[bookmark: _Hlk194577698]SAMPLING AND TESTING OF WATER & WASTEWATER SAMPLES

SPECIFICATIONS

1. SCOPE OF SUPPLY OF SERVICE/GOODS

Sampling and testing of potable and waste water samples in the Kannaland Local Municipality area for a period of three (3) months from April 2025 – June 2025.

2. SPECIFICATIONS REQUIREMENTS

2.1 Receiving samples

· All procured samples within Kannaland Municipal area must be collected at the office of the area where the samples were taken, as indicated in Annexure C.
· Upon receipt of the samples it would be expected of the service provider to check on the physical state of all samples and to take temperature measurements of the samples received.
· The service provider should ensure that where applicable samples are kept within the appropriate temperature ranges. Samples not conforming to the temperature ranges and other criteria must be left at the office.


2.2 Analysis of samples

· Where possible, actual sampling results must be indicated; if this in not achievable, the maximum results that can be provided must be indicated.
2.3 Sample results

· Bacteriological results must be provided within five (5) days of submission for analysis or any longer period as decided between the two parties beforehand.
· Chemical water sample results must be provided within ten (10) days of submission for samples analyse.
· Results should be emailed to the contact person or persons that will be nominated by Kannaland Municipality

2.4 Containers and sampling material

· It will be expected of the service provider to provide an adequate number of sampling containers (cooler boxes and ice packs) and bottles of appropriate sizes. These need to be available to Kannaland Municipality for different sample types at the different offices in Ladismith, Calitzdorp, Zoar and Van Wyksdorp.
· Sample containers for the monitoring of chlorinated water e.g. drinking water and chlorine treated waste water must contain Sodium Thiosulphate crystals in order to neutralize all traces of chlorine in the water
· The service provider should provide sterile swabs for surface and other samples as well as sterile containers for these swabs


2.5 Labels

· Labels must be provided for each sample container.
· The label must have enough space for the Process Controller to write the sample identification number, name of the Process Controller and sample type
· These labels must be provided with adhesive at the back and must e able to stick to the sample container.

2.6 Seals
· Seals need to be provided for each container that could be used by the Process Controller to secure the content of the container.
· Each seal should bear a unique sample number.

3. Total Samples

3.1 Receiving samples: Water

See attached Annexure A

3.2 Receiving samples: Wastewater

See attached Annexure B


CRITERIA FOR BIDDERS – MINIMUM REQUIREMENTS

	ITEM
	DESCRIPTION
	YES
	NO

	1.
	Laboratory must be SANAS approved and a certificate of proof of registration provided.

	
	

	2.
	The bidder must have a registered office within 200km from the Municipal Head Office in Ladismith.

	
	

	3.
	The bidder must ensure that transport costs of samples and the return of cooler boxes and ice packs to Kannaland Municipality in Ladismith, Calitzdorp, Zoar and Van Wyksdorp is included in the quotation as part of the analytical costs.

	
	

	4.
	The bidder must supply sterilized water containers (bottles) for the sampling of water and other liquids for bacteriological analysis. Sample containers for the monitoring of chlorinated water must contain Sodium Thiosulphate crystals to in order to neutralize all traces of chlorine in water. Chemicals sample containers must have a capacity needed for analysis of the sample type.

	
	

	5.
	All prices must include VAT if you are a VAT vendor.

	
	





PRICING SCHEDULE

	NO
	DESCRIPTION
	QTY
	UNIT
	RATE
	AMOUNT

	1
	All-inclusive price for sampling and testing of water and waste water as per specifications and requirements

	
	
	
	

	
	a) Water sampling and testing
	1
	Sum
	
	

	
	b) Wastewater sampling and testing
	1
	Sum
	
	

	
	
	
	
	
	

	
	Total Excl. VAT
	

	
	VAT @ 15%
	

	
	Total Incl. VAT
	





Annexure A – Water sampling (All towns)
[image: ]

Annexure B – Wastewater sampling
[image: ]
Annexure C – Locality Map

	
Site Locality
	
GPS Coordinates

	
GPS Coordinates


	Calitzdorp

	-33.5309773
	21.689954

	Zoar

	-33.496189
	21.448353

	Ladismith

	-33.4945364
	21.263823

	Van Wyksdorp

	-33.748836
	21.459751
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ANNEXURE A

WATER SAMPLING

TYPE DETERMINAND

W14 W15 W16 W17 W18

TOTAL (APR 2025)

W19 W20 W21 W22

TOTAL (MAY 2025)

W23 W24 W25 W26

TOTAL (JUNE 2025)

TOTAL (QUARTER 3)

Water  Electrical Conductivity 6 6 6 6 6 6 18

Water  pH at 25 

o

C 6 6 2 14 6 8 14 6 8 14 42

Water  Turbidity 8 8 16 8 8 16 8 8 16 48

Water  Free Chlorine 8 8 16 8 8 16 8 8 16 48

Water  E.Coli 3 5 3 5 6 22 3 5 3 8 19 3 5 3 8 19 60

Water  Coliforms 4 4 4 4 8 24 4 4 4 8 20 4 4 4 8 20 64

Water  Heterotropic Plate Count 1 7 1 7 2 18 1 7 1 8 17 1 7 1 8 17 52

Water  Iron as Fe 2 2 3 7 2 5 7 2 5 7 21

Water  Nitrate as N 4 4 4 4 4 4 12

Water  Nitrate as N 4 4 4 4 4 4 12

Water  Sulphate as SO

4

 

2-

4 4 4 4 4 4 12

Water  Fluoride as F- 4 4 4 4 4 4 12

Water  Boron as B 4 4 4 4 4 4 12

Water  Copper as Cu 4 4 4 4 4 4 12

Water  Manganese as Mn 4 4 4 4 4 4 12

Water  Total Dissolved Solids at 180 

o

C 4 4 4 4 4 4 12

Water  Ammonia as N 4 4 4 4 4 4 12

Water  Chloride as Cl 4 4 4 4 4 4 12

Water  Sodium as Na 4 4 4 4 4 4 12

Water  Zinc as Zn 4 4 4 4 4 4 12

Water  Calcium as Ca 4 4 4 4 4 4 12

Water  Magnesium as Mg 4 4 4 4 4 4 12

Water  Potassium as K 4 4 4 4 4 4 12

Water  Aluminium as Al 3 3 3 3 4 16 3 3 3 4 13 3 3 3 4 13 42

TOTA L 11 43 11 43 91 199 11 43 11 123 188 11 43 11 123 188 575
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ANNEXURE B

WATER SAMPLING

TYPE DETERMINAND

W14 W15 W16 W17 W18

TOTAL (APR 2025)

W19 W20 W21 W22

TOTAL (MAY 2025)

W23 W24 W25 W26

TOTAL (JUNE 2025)

TOTAL (QUARTER 3)

WastewaterElectrical Conductivity 4 4 4 4 4 4 12

WastewaterpH at 25 

o

C 4 4 4 4 4 4 12

WastewaterFree Chlorine 4 4 4 4 4 4 12

WastewaterAmmonia as N 4 4 4 4 4 4 12

WastewaterTotal chlorine 4 4 4 4 4 4 12

WastewaterOrtho-Phosphate as P 4 4 4 4 4 4 12

WastewaterTotal Suspended Solids 4 4 4 4 4 4 12

WastewaterFats, Oils, & Grease 4 4 4 4 4 4 12

WastewaterChemical Oxygen Demand 4 4 4 4 4 4 12

WastewaterCourier Fee 4 4 4 4 4 4 12

WastewaterFaecal Coliforms 4 4 4 4 4 4 12

TOTA L 0 0 0 0 44 44 0 0 0 44 44 0 0 0 44 44 132


