{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["ANNEXURE A PRICING SCHEDULE"],"not_rendered":{"images":1,"defined_names":3},"read":"whole","date_system":"1900"}

{"sheet":"ANNEXURE A PRICING SCHEDULE","index":0,"n_rows":681,"n_cols":27,"rows_kept":681}
[]
[]
[{"$nulls":4},"RT74-2027:  ANNEXURE A PRICING SCHEDULE"]
[]
[]
["#","Item Number","Group Series","Category","Item Description","Province","Bidder Name","Brand Name","Pricing in Rands \nincluding delivery costs and VAT","Name of the Original Manufacturer","Country of Orgigin","Foreign Currency Name","Local Production and Content %","Import Percentage","Minimum Order Quantity","Product Code Number","Delivery Period (Days)",null,"D1 – Imported Raw Material / Finished product ","D2 - Local Raw Material / Finished product (if applicable) ","D3 – Labour ","D4 – Transport ","D5 – Overheads  ","D6 – Other ","D4 – Transport ","D5 – Overheads  ","D6 – Other "]
[1,"RT74-01-001","Group Series 1","Clip Type Shelving","ADDITIONAL SHELF FOR CLIP TYPE SHELVING UNIT\nSize 914mm wide x 305mm deep. 1mm thick cold rolled commercial quality steel\nUniformly distributed mass load of 170kg \nTo comply with CKS 370 standard\nThis item is additional to the below items:\nRT74-01-002,RT74-01-003,RT74-01-004,RT74-01-005","Eastern Cape"]
[2,"RT74-01-001","Group Series 1","Clip Type Shelving","ADDITIONAL SHELF FOR CLIP TYPE SHELVING UNIT\nSize 914mm wide x 305mm deep. 1mm thick cold rolled commercial quality steel\nUniformly distributed mass load of 170kg \nTo comply with CKS 370 standard\nThis item is additional to the below items:\nRT74-01-002,RT74-01-003,RT74-01-004,RT74-01-005","Free State"]
[3,"RT74-01-001","Group Series 1","Clip Type Shelving","ADDITIONAL SHELF FOR CLIP TYPE SHELVING UNIT\nSize 914mm wide x 305mm deep. 1mm thick cold rolled commercial quality steel\nUniformly distributed mass load of 170kg \nTo comply with CKS 370 standard\nThis item is additional to the below items:\nRT74-01-002,RT74-01-003,RT74-01-004,RT74-01-005","Gauteng"]
[4,"RT74-01-001","Group Series 1","Clip Type Shelving","ADDITIONAL SHELF FOR CLIP TYPE SHELVING UNIT\nSize 914mm wide x 305mm deep. 1mm thick cold rolled commercial quality steel\nUniformly distributed mass load of 170kg \nTo comply with CKS 370 standard\nThis item is additional to the below items:\nRT74-01-002,RT74-01-003,RT74-01-004,RT74-01-005","Kwazulu-Natal"]
[5,"RT74-01-001","Group Series 1","Clip Type Shelving","ADDITIONAL SHELF FOR CLIP TYPE SHELVING UNIT\nSize 914mm wide x 305mm deep. 1mm thick cold rolled commercial quality steel\nUniformly distributed mass load of 170kg \nTo comply with CKS 370 standard\nThis item is additional to the below items:\nRT74-01-002,RT74-01-003,RT74-01-004,RT74-01-005","Limpopo"]
[6,"RT74-01-001","Group Series 1","Clip Type Shelving","ADDITIONAL SHELF FOR CLIP TYPE SHELVING UNIT\nSize 914mm wide x 305mm deep. 1mm thick cold rolled commercial quality steel\nUniformly distributed mass load of 170kg \nTo comply with CKS 370 standard\nThis item is additional to the below items:\nRT74-01-002,RT74-01-003,RT74-01-004,RT74-01-005","Mpumalanga"]
[7,"RT74-01-001","Group Series 1","Clip Type Shelving","ADDITIONAL SHELF FOR CLIP TYPE SHELVING UNIT\nSize 914mm wide x 305mm deep. 1mm thick cold rolled commercial quality steel\nUniformly distributed mass load of 170kg \nTo comply with CKS 370 standard\nThis item is additional to the below items:\nRT74-01-002,RT74-01-003,RT74-01-004,RT74-01-005","Northern Cape"]
[8,"RT74-01-001","Group Series 1","Clip Type Shelving","ADDITIONAL SHELF FOR CLIP TYPE SHELVING UNIT\nSize 914mm wide x 305mm deep. 1mm thick cold rolled commercial quality steel\nUniformly distributed mass load of 170kg \nTo comply with CKS 370 standard\nThis item is additional to the below items:\nRT74-01-002,RT74-01-003,RT74-01-004,RT74-01-005","North West"]
[9,"RT74-01-001","Group Series 1","Clip Type Shelving","ADDITIONAL SHELF FOR CLIP TYPE SHELVING UNIT\nSize 914mm wide x 305mm deep. 1mm thick cold rolled commercial quality steel\nUniformly distributed mass load of 170kg \nTo comply with CKS 370 standard\nThis item is additional to the below items:\nRT74-01-002,RT74-01-003,RT74-01-004,RT74-01-005","Western Cape"]
[10,"RT74-01-002","Group Series 1","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Eastern Cape"]
[11,"RT74-01-002","Group Series 1","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Free State"]
[12,"RT74-01-002","Group Series 1","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Gauteng"]
[13,"RT74-01-002","Group Series 1","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Kwazulu-Natal"]
[14,"RT74-01-002","Group Series 1","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Limpopo"]
[15,"RT74-01-002","Group Series 1","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Mpumalanga"]
[16,"RT74-01-002","Group Series 1","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Northern Cape"]
[17,"RT74-01-002","Group Series 1","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","North West"]
[18,"RT74-01-002","Group Series 1","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Western Cape"]
[19,"RT74-01-003","Group Series 1","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Eastern Cape"]
[20,"RT74-01-003","Group Series 1","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Free State"]
[21,"RT74-01-003","Group Series 1","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Gauteng"]
[22,"RT74-01-003","Group Series 1","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Kwazulu-Natal"]
[23,"RT74-01-003","Group Series 1","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Limpopo"]
[24,"RT74-01-003","Group Series 1","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Mpumalanga"]
[25,"RT74-01-003","Group Series 1","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Northern Cape"]
[26,"RT74-01-003","Group Series 1","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","North West"]
[27,"RT74-01-003","Group Series 1","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Western Cape"]
[28,"RT74-01-004","Group Series 1","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Eastern Cape"]
[29,"RT74-01-004","Group Series 1","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Free State"]
[30,"RT74-01-004","Group Series 1","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Gauteng"]
[31,"RT74-01-004","Group Series 1","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Kwazulu-Natal"]
[32,"RT74-01-004","Group Series 1","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Limpopo"]
[33,"RT74-01-004","Group Series 1","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Mpumalanga"]
[34,"RT74-01-004","Group Series 1","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Northern Cape"]
[35,"RT74-01-004","Group Series 1","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","North West"]
[36,"RT74-01-004","Group Series 1","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Western Cape"]
[37,"RT74-01-005","Group Series 1","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\n Size 2210mm high x 914mm wide x 305mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Eastern Cape"]
[38,"RT74-01-005","Group Series 1","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\n Size 2210mm high x 914mm wide x 305mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Free State"]
[39,"RT74-01-005","Group Series 1","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\n Size 2210mm high x 914mm wide x 305mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Gauteng"]
[40,"RT74-01-005","Group Series 1","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\n Size 2210mm high x 914mm wide x 305mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Kwazulu-Natal"]
[41,"RT74-01-005","Group Series 1","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\n Size 2210mm high x 914mm wide x 305mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Limpopo"]
[42,"RT74-01-005","Group Series 1","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\n Size 2210mm high x 914mm wide x 305mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Mpumalanga"]
[43,"RT74-01-005","Group Series 1","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\n Size 2210mm high x 914mm wide x 305mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Northern Cape"]
[44,"RT74-01-005","Group Series 1","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\n Size 2210mm high x 914mm wide x 305mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","North West"]
[45,"RT74-01-005","Group Series 1","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\n Size 2210mm high x 914mm wide x 305mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Western Cape"]
[46,"RT74-01-006","Group Series 2","Clip Type Shelving","ADDITIONAL SHELF FOR CLIP TYPE SHELVING UNIT\n Size 914mm wide x 381mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items \nRT74-01-007,RT74-01-008,RT74-01-009,RT74-01-010","Eastern Cape"]
[47,"RT74-01-006","Group Series 2","Clip Type Shelving","ADDITIONAL SHELF FOR CLIP TYPE SHELVING UNIT\n Size 914mm wide x 381mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items \nRT74-01-007,RT74-01-008,RT74-01-009,RT74-01-010","Free State"]
[48,"RT74-01-006","Group Series 2","Clip Type Shelving","ADDITIONAL SHELF FOR CLIP TYPE SHELVING UNIT\n Size 914mm wide x 381mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items \nRT74-01-007,RT74-01-008,RT74-01-009,RT74-01-010","Gauteng"]
[49,"RT74-01-006","Group Series 2","Clip Type Shelving","ADDITIONAL SHELF FOR CLIP TYPE SHELVING UNIT\n Size 914mm wide x 381mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items \nRT74-01-007,RT74-01-008,RT74-01-009,RT74-01-010","Kwazulu-Natal"]
[50,"RT74-01-006","Group Series 2","Clip Type Shelving","ADDITIONAL SHELF FOR CLIP TYPE SHELVING UNIT\n Size 914mm wide x 381mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items \nRT74-01-007,RT74-01-008,RT74-01-009,RT74-01-010","Limpopo"]
[51,"RT74-01-006","Group Series 2","Clip Type Shelving","ADDITIONAL SHELF FOR CLIP TYPE SHELVING UNIT\n Size 914mm wide x 381mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items \nRT74-01-007,RT74-01-008,RT74-01-009,RT74-01-010","Mpumalanga"]
[52,"RT74-01-006","Group Series 2","Clip Type Shelving","ADDITIONAL SHELF FOR CLIP TYPE SHELVING UNIT\n Size 914mm wide x 381mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items \nRT74-01-007,RT74-01-008,RT74-01-009,RT74-01-010","Northern Cape"]
[53,"RT74-01-006","Group Series 2","Clip Type Shelving","ADDITIONAL SHELF FOR CLIP TYPE SHELVING UNIT\n Size 914mm wide x 381mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items \nRT74-01-007,RT74-01-008,RT74-01-009,RT74-01-010","North West"]
[54,"RT74-01-006","Group Series 2","Clip Type Shelving","ADDITIONAL SHELF FOR CLIP TYPE SHELVING UNIT\n Size 914mm wide x 381mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items \nRT74-01-007,RT74-01-008,RT74-01-009,RT74-01-010","Western Cape"]
[55,"RT74-01-007","Group Series 2","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS\nSize 1905mm high x 914mm wide x 381mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel \nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Eastern Cape"]
[56,"RT74-01-007","Group Series 2","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS\nSize 1905mm high x 914mm wide x 381mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel \nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Free State"]
[57,"RT74-01-007","Group Series 2","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS\nSize 1905mm high x 914mm wide x 381mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel \nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Gauteng"]
[58,"RT74-01-007","Group Series 2","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS\nSize 1905mm high x 914mm wide x 381mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel \nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Kwazulu-Natal"]
[59,"RT74-01-007","Group Series 2","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS\nSize 1905mm high x 914mm wide x 381mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel \nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Limpopo"]
[60,"RT74-01-007","Group Series 2","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS\nSize 1905mm high x 914mm wide x 381mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel \nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Mpumalanga"]
[61,"RT74-01-007","Group Series 2","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS\nSize 1905mm high x 914mm wide x 381mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel \nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Northern Cape"]
[62,"RT74-01-007","Group Series 2","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS\nSize 1905mm high x 914mm wide x 381mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel \nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","North West"]
[63,"RT74-01-007","Group Series 2","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS\nSize 1905mm high x 914mm wide x 381mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel \nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Western Cape"]
[64,"RT74-01-008","Group Series 2","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\n Size 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel. \nUniformly distributed mass load of 170kg per shelf. \nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Eastern Cape"]
[65,"RT74-01-008","Group Series 2","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\n Size 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel. \nUniformly distributed mass load of 170kg per shelf. \nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Free State"]
[66,"RT74-01-008","Group Series 2","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\n Size 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel. \nUniformly distributed mass load of 170kg per shelf. \nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Gauteng"]
[67,"RT74-01-008","Group Series 2","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\n Size 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel. \nUniformly distributed mass load of 170kg per shelf. \nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Kwazulu-Natal"]
[68,"RT74-01-008","Group Series 2","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\n Size 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel. \nUniformly distributed mass load of 170kg per shelf. \nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Limpopo"]
[69,"RT74-01-008","Group Series 2","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\n Size 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel. \nUniformly distributed mass load of 170kg per shelf. \nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Mpumalanga"]
[70,"RT74-01-008","Group Series 2","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\n Size 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel. \nUniformly distributed mass load of 170kg per shelf. \nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Northern Cape"]
[71,"RT74-01-008","Group Series 2","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\n Size 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel. \nUniformly distributed mass load of 170kg per shelf. \nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","North West"]
[72,"RT74-01-008","Group Series 2","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\n Size 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel. \nUniformly distributed mass load of 170kg per shelf. \nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Western Cape"]
[73,"RT74-01-009","Group Series 2","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS\n Size 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel. \nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves \nTo comply with CKS 370 standard","Eastern Cape"]
[74,"RT74-01-009","Group Series 2","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS\n Size 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel. \nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves \nTo comply with CKS 370 standard","Free State"]
[75,"RT74-01-009","Group Series 2","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS\n Size 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel. \nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves \nTo comply with CKS 370 standard","Gauteng"]
[76,"RT74-01-009","Group Series 2","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS\n Size 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel. \nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves \nTo comply with CKS 370 standard","Kwazulu-Natal"]
[77,"RT74-01-009","Group Series 2","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS\n Size 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel. \nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves \nTo comply with CKS 370 standard","Limpopo"]
[78,"RT74-01-009","Group Series 2","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS\n Size 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel. \nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves \nTo comply with CKS 370 standard","Mpumalanga"]
[79,"RT74-01-009","Group Series 2","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS\n Size 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel. \nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves \nTo comply with CKS 370 standard","Northern Cape"]
[80,"RT74-01-009","Group Series 2","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS\n Size 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel. \nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves \nTo comply with CKS 370 standard","North West"]
[81,"RT74-01-009","Group Series 2","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS\n Size 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel. \nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves \nTo comply with CKS 370 standard","Western Cape"]
[82,"RT74-01-010","Group Series 2","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\n Size 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel. \nUniformly distributed mass load of 170kg per shelf. \nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Eastern Cape"]
[83,"RT74-01-010","Group Series 2","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\n Size 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel. \nUniformly distributed mass load of 170kg per shelf. \nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Free State"]
[84,"RT74-01-010","Group Series 2","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\n Size 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel. \nUniformly distributed mass load of 170kg per shelf. \nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Gauteng"]
[85,"RT74-01-010","Group Series 2","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\n Size 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel. \nUniformly distributed mass load of 170kg per shelf. \nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Kwazulu-Natal"]
[86,"RT74-01-010","Group Series 2","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\n Size 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel. \nUniformly distributed mass load of 170kg per shelf. \nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Limpopo"]
[87,"RT74-01-010","Group Series 2","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\n Size 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel. \nUniformly distributed mass load of 170kg per shelf. \nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Mpumalanga"]
[88,"RT74-01-010","Group Series 2","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\n Size 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel. \nUniformly distributed mass load of 170kg per shelf. \nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Northern Cape"]
[89,"RT74-01-010","Group Series 2","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\n Size 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel. \nUniformly distributed mass load of 170kg per shelf. \nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","North West"]
[90,"RT74-01-010","Group Series 2","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\n Size 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel. \nUniformly distributed mass load of 170kg per shelf. \nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Western Cape"]
[91,"RT74-01-011","Group Series 3","Clip Type Shelving","ADDITIONAL SHELF FOR CLIP TYPE SHELVING UNIT\nSize 914mm wide x 457mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items \nRT74-01-012,RT74-01-013,RT74-01-014,RT74-01-015","Eastern Cape"]
[92,"RT74-01-011","Group Series 3","Clip Type Shelving","ADDITIONAL SHELF FOR CLIP TYPE SHELVING UNIT\nSize 914mm wide x 457mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items \nRT74-01-012,RT74-01-013,RT74-01-014,RT74-01-015","Free State"]
[93,"RT74-01-011","Group Series 3","Clip Type Shelving","ADDITIONAL SHELF FOR CLIP TYPE SHELVING UNIT\nSize 914mm wide x 457mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items \nRT74-01-012,RT74-01-013,RT74-01-014,RT74-01-015","Gauteng"]
[94,"RT74-01-011","Group Series 3","Clip Type Shelving","ADDITIONAL SHELF FOR CLIP TYPE SHELVING UNIT\nSize 914mm wide x 457mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items \nRT74-01-012,RT74-01-013,RT74-01-014,RT74-01-015","Kwazulu-Natal"]
[95,"RT74-01-011","Group Series 3","Clip Type Shelving","ADDITIONAL SHELF FOR CLIP TYPE SHELVING UNIT\nSize 914mm wide x 457mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items \nRT74-01-012,RT74-01-013,RT74-01-014,RT74-01-015","Limpopo"]
[96,"RT74-01-011","Group Series 3","Clip Type Shelving","ADDITIONAL SHELF FOR CLIP TYPE SHELVING UNIT\nSize 914mm wide x 457mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items \nRT74-01-012,RT74-01-013,RT74-01-014,RT74-01-015","Mpumalanga"]
[97,"RT74-01-011","Group Series 3","Clip Type Shelving","ADDITIONAL SHELF FOR CLIP TYPE SHELVING UNIT\nSize 914mm wide x 457mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items \nRT74-01-012,RT74-01-013,RT74-01-014,RT74-01-015","Northern Cape"]
[98,"RT74-01-011","Group Series 3","Clip Type Shelving","ADDITIONAL SHELF FOR CLIP TYPE SHELVING UNIT\nSize 914mm wide x 457mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items \nRT74-01-012,RT74-01-013,RT74-01-014,RT74-01-015","North West"]
[99,"RT74-01-011","Group Series 3","Clip Type Shelving","ADDITIONAL SHELF FOR CLIP TYPE SHELVING UNIT\nSize 914mm wide x 457mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items \nRT74-01-012,RT74-01-013,RT74-01-014,RT74-01-015","Western Cape"]
[100,"RT74-01-012","Group Series 3","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS\nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Eastern Cape"]
[101,"RT74-01-012","Group Series 3","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS\nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Free State"]
[102,"RT74-01-012","Group Series 3","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS\nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Gauteng"]
[103,"RT74-01-012","Group Series 3","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS\nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Kwazulu-Natal"]
[104,"RT74-01-012","Group Series 3","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS\nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Limpopo"]
[105,"RT74-01-012","Group Series 3","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS\nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Mpumalanga"]
[106,"RT74-01-012","Group Series 3","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS\nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Northern Cape"]
[107,"RT74-01-012","Group Series 3","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS\nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","North West"]
[108,"RT74-01-012","Group Series 3","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS\nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Western Cape"]
[109,"RT74-01-013","Group Series 3","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel. \nUniformly distributed mass load of 170kg per shelf. \nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Eastern Cape"]
[110,"RT74-01-013","Group Series 3","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel. \nUniformly distributed mass load of 170kg per shelf. \nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Free State"]
[111,"RT74-01-013","Group Series 3","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel. \nUniformly distributed mass load of 170kg per shelf. \nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Gauteng"]
[112,"RT74-01-013","Group Series 3","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel. \nUniformly distributed mass load of 170kg per shelf. \nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Kwazulu-Natal"]
[113,"RT74-01-013","Group Series 3","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel. \nUniformly distributed mass load of 170kg per shelf. \nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Limpopo"]
[114,"RT74-01-013","Group Series 3","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel. \nUniformly distributed mass load of 170kg per shelf. \nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Mpumalanga"]
[115,"RT74-01-013","Group Series 3","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel. \nUniformly distributed mass load of 170kg per shelf. \nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Northern Cape"]
[116,"RT74-01-013","Group Series 3","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel. \nUniformly distributed mass load of 170kg per shelf. \nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","North West"]
[117,"RT74-01-013","Group Series 3","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel. \nUniformly distributed mass load of 170kg per shelf. \nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Western Cape"]
[118,"RT74-01-014","Group Series 3","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS. \nSize 2210mm high x 914mm wide x 457mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel. \nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Eastern Cape"]
[119,"RT74-01-014","Group Series 3","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS. \nSize 2210mm high x 914mm wide x 457mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel. \nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Free State"]
[120,"RT74-01-014","Group Series 3","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS. \nSize 2210mm high x 914mm wide x 457mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel. \nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Gauteng"]
[121,"RT74-01-014","Group Series 3","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS. \nSize 2210mm high x 914mm wide x 457mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel. \nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Kwazulu-Natal"]
[122,"RT74-01-014","Group Series 3","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS. \nSize 2210mm high x 914mm wide x 457mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel. \nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Limpopo"]
[123,"RT74-01-014","Group Series 3","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS. \nSize 2210mm high x 914mm wide x 457mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel. \nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Mpumalanga"]
[124,"RT74-01-014","Group Series 3","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS. \nSize 2210mm high x 914mm wide x 457mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel. \nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Northern Cape"]
[125,"RT74-01-014","Group Series 3","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS. \nSize 2210mm high x 914mm wide x 457mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel. \nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","North West"]
[126,"RT74-01-014","Group Series 3","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS. \nSize 2210mm high x 914mm wide x 457mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel. \nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Western Cape"]
[127,"RT74-01-015","Group Series 3","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 2210mm high x 914mm wide x 457mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Eastern Cape"]
[128,"RT74-01-015","Group Series 3","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 2210mm high x 914mm wide x 457mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Free State"]
[129,"RT74-01-015","Group Series 3","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 2210mm high x 914mm wide x 457mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Gauteng"]
[130,"RT74-01-015","Group Series 3","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 2210mm high x 914mm wide x 457mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Kwazulu-Natal"]
[131,"RT74-01-015","Group Series 3","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 2210mm high x 914mm wide x 457mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Limpopo"]
[132,"RT74-01-015","Group Series 3","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 2210mm high x 914mm wide x 457mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Mpumalanga"]
[133,"RT74-01-015","Group Series 3","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 2210mm high x 914mm wide x 457mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Northern Cape"]
[134,"RT74-01-015","Group Series 3","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 2210mm high x 914mm wide x 457mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","North West"]
[135,"RT74-01-015","Group Series 3","Clip Type Shelving","CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 2210mm high x 914mm wide x 457mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Western Cape"]
[136,"RT74-02-001","Group Series 4","Beaded Type Shelving","ADDITIONAL SHELF FOR BEADED TYPE SHELVING UNIT\nSize 914mm wide x 305mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items :\nRT74-02-002,RT74-02-003,RT74-02-004,RT74-02-005\n","Eastern Cape"]
[137,"RT74-02-001","Group Series 4","Beaded Type Shelving","ADDITIONAL SHELF FOR BEADED TYPE SHELVING UNIT\nSize 914mm wide x 305mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items :\nRT74-02-002,RT74-02-003,RT74-02-004,RT74-02-005\n","Free State"]
[138,"RT74-02-001","Group Series 4","Beaded Type Shelving","ADDITIONAL SHELF FOR BEADED TYPE SHELVING UNIT\nSize 914mm wide x 305mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items :\nRT74-02-002,RT74-02-003,RT74-02-004,RT74-02-005\n","Gauteng"]
[139,"RT74-02-001","Group Series 4","Beaded Type Shelving","ADDITIONAL SHELF FOR BEADED TYPE SHELVING UNIT\nSize 914mm wide x 305mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items :\nRT74-02-002,RT74-02-003,RT74-02-004,RT74-02-005\n","Kwazulu-Natal"]
[140,"RT74-02-001","Group Series 4","Beaded Type Shelving","ADDITIONAL SHELF FOR BEADED TYPE SHELVING UNIT\nSize 914mm wide x 305mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items :\nRT74-02-002,RT74-02-003,RT74-02-004,RT74-02-005\n","Limpopo"]
[141,"RT74-02-001","Group Series 4","Beaded Type Shelving","ADDITIONAL SHELF FOR BEADED TYPE SHELVING UNIT\nSize 914mm wide x 305mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items :\nRT74-02-002,RT74-02-003,RT74-02-004,RT74-02-005\n","Mpumalanga"]
[142,"RT74-02-001","Group Series 4","Beaded Type Shelving","ADDITIONAL SHELF FOR BEADED TYPE SHELVING UNIT\nSize 914mm wide x 305mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items :\nRT74-02-002,RT74-02-003,RT74-02-004,RT74-02-005\n","Northern Cape"]
[143,"RT74-02-001","Group Series 4","Beaded Type Shelving","ADDITIONAL SHELF FOR BEADED TYPE SHELVING UNIT\nSize 914mm wide x 305mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items :\nRT74-02-002,RT74-02-003,RT74-02-004,RT74-02-005\n","North West"]
[144,"RT74-02-001","Group Series 4","Beaded Type Shelving","ADDITIONAL SHELF FOR BEADED TYPE SHELVING UNIT\nSize 914mm wide x 305mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items :\nRT74-02-002,RT74-02-003,RT74-02-004,RT74-02-005\n","Western Cape"]
[145,"RT74-02-002","Group Series 4","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Eastern Cape"]
[146,"RT74-02-002","Group Series 4","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Free State"]
[147,"RT74-02-002","Group Series 4","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Gauteng"]
[148,"RT74-02-002","Group Series 4","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Kwazulu-Natal"]
[149,"RT74-02-002","Group Series 4","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Limpopo"]
[150,"RT74-02-002","Group Series 4","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Mpumalanga"]
[151,"RT74-02-002","Group Series 4","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Northern Cape"]
[152,"RT74-02-002","Group Series 4","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","North West"]
[153,"RT74-02-002","Group Series 4","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Western Cape"]
[154,"RT74-02-003","Group Series 4","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Eastern Cape"]
[155,"RT74-02-003","Group Series 4","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Free State"]
[156,"RT74-02-003","Group Series 4","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Gauteng"]
[157,"RT74-02-003","Group Series 4","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Kwazulu-Natal"]
[158,"RT74-02-003","Group Series 4","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Limpopo"]
[159,"RT74-02-003","Group Series 4","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Mpumalanga"]
[160,"RT74-02-003","Group Series 4","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Northern Cape"]
[161,"RT74-02-003","Group Series 4","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","North West"]
[162,"RT74-02-003","Group Series 4","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Western Cape"]
[163,"RT74-02-004","Group Series 4","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 2210mm high x 914mm wide x 305mm deep. 7 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard\n","Eastern Cape"]
[164,"RT74-02-004","Group Series 4","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 2210mm high x 914mm wide x 305mm deep. 7 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard\n","Free State"]
[165,"RT74-02-004","Group Series 4","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 2210mm high x 914mm wide x 305mm deep. 7 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard\n","Gauteng"]
[166,"RT74-02-004","Group Series 4","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 2210mm high x 914mm wide x 305mm deep. 7 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard\n","Kwazulu-Natal"]
[167,"RT74-02-004","Group Series 4","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 2210mm high x 914mm wide x 305mm deep. 7 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Limpopo"]
[168,"RT74-02-004","Group Series 4","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 2210mm high x 914mm wide x 305mm deep. 7 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard\n","Mpumalanga"]
[169,"RT74-02-004","Group Series 4","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 2210mm high x 914mm wide x 305mm deep. 7 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard\n","Northern Cape"]
[170,"RT74-02-004","Group Series 4","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 2210mm high x 914mm wide x 305mm deep. 7 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard\n","North West"]
[171,"RT74-02-004","Group Series 4","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 2210mm high x 914mm wide x 305mm deep. 7 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard\n","Western Cape"]
[172,"RT74-02-005","Group Series 4","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 2210mm high x 914mm wide x 305mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Eastern Cape"]
[173,"RT74-02-005","Group Series 4","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 2210mm high x 914mm wide x 305mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Free State"]
[174,"RT74-02-005","Group Series 4","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 2210mm high x 914mm wide x 305mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Gauteng"]
[175,"RT74-02-005","Group Series 4","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 2210mm high x 914mm wide x 305mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Kwazulu-Natal"]
[176,"RT74-02-005","Group Series 4","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 2210mm high x 914mm wide x 305mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Limpopo"]
[177,"RT74-02-005","Group Series 4","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 2210mm high x 914mm wide x 305mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Mpumalanga"]
[178,"RT74-02-005","Group Series 4","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 2210mm high x 914mm wide x 305mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Northern Cape"]
[179,"RT74-02-005","Group Series 4","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 2210mm high x 914mm wide x 305mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","North West"]
[180,"RT74-02-005","Group Series 4","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 2210mm high x 914mm wide x 305mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Western Cape"]
[181,"RT74-02-006","Group Series 5","Beaded Type Shelving","ADDITIONAL SHELF FOR BEADED TYPE SHELVING UNIT\nSize 914mm wide x 381mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items :\nRT74-02-007,RT74-02-008,RT74-02-009,RT74-02-010","Eastern Cape"]
[182,"RT74-02-006","Group Series 5","Beaded Type Shelving","ADDITIONAL SHELF FOR BEADED TYPE SHELVING UNIT\nSize 914mm wide x 381mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items :\nRT74-02-007,RT74-02-008,RT74-02-009,RT74-02-010","Free State"]
[183,"RT74-02-006","Group Series 5","Beaded Type Shelving","ADDITIONAL SHELF FOR BEADED TYPE SHELVING UNIT\nSize 914mm wide x 381mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items :\nRT74-02-007,RT74-02-008,RT74-02-009,RT74-02-010","Gauteng"]
[184,"RT74-02-006","Group Series 5","Beaded Type Shelving","ADDITIONAL SHELF FOR BEADED TYPE SHELVING UNIT\nSize 914mm wide x 381mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items :\nRT74-02-007,RT74-02-008,RT74-02-009,RT74-02-010","Kwazulu-Natal"]
[185,"RT74-02-006","Group Series 5","Beaded Type Shelving","ADDITIONAL SHELF FOR BEADED TYPE SHELVING UNIT\nSize 914mm wide x 381mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standardThis item is additional to the below items :\nRT74-02-007,RT74-02-008,RT74-02-009,RT74-02-010","Limpopo"]
[186,"RT74-02-006","Group Series 5","Beaded Type Shelving","ADDITIONAL SHELF FOR BEADED TYPE SHELVING UNIT\nSize 914mm wide x 381mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items :\nRT74-02-007,RT74-02-008,RT74-02-009,RT74-02-010","Mpumalanga"]
[187,"RT74-02-006","Group Series 5","Beaded Type Shelving","ADDITIONAL SHELF FOR BEADED TYPE SHELVING UNIT\nSize 914mm wide x 381mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items :\nRT74-02-007,RT74-02-008,RT74-02-009,RT74-02-010","Northern Cape"]
[188,"RT74-02-006","Group Series 5","Beaded Type Shelving","ADDITIONAL SHELF FOR BEADED TYPE SHELVING UNIT\nSize 914mm wide x 381mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items :\nRT74-02-007,RT74-02-008,RT74-02-009,RT74-02-010","North West"]
[189,"RT74-02-006","Group Series 5","Beaded Type Shelving","ADDITIONAL SHELF FOR BEADED TYPE SHELVING UNIT\nSize 914mm wide x 381mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items :\nRT74-02-007,RT74-02-008,RT74-02-009,RT74-02-010","Western Cape"]
[190,"RT74-02-007","Group Series 5","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING.\nSize 1905mm high x 914mm wide x 381mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Eastern Cape"]
[191,"RT74-02-007","Group Series 5","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING.\nSize 1905mm high x 914mm wide x 381mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Free State"]
[192,"RT74-02-007","Group Series 5","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING.\nSize 1905mm high x 914mm wide x 381mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Gauteng"]
[193,"RT74-02-007","Group Series 5","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING.\nSize 1905mm high x 914mm wide x 381mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Kwazulu-Natal"]
[194,"RT74-02-007","Group Series 5","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING.\nSize 1905mm high x 914mm wide x 381mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Limpopo"]
[195,"RT74-02-007","Group Series 5","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING.\nSize 1905mm high x 914mm wide x 381mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Mpumalanga"]
[196,"RT74-02-007","Group Series 5","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING.\nSize 1905mm high x 914mm wide x 381mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Northern Cape"]
[197,"RT74-02-007","Group Series 5","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING.\nSize 1905mm high x 914mm wide x 381mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","North West"]
[198,"RT74-02-007","Group Series 5","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING.\nSize 1905mm high x 914mm wide x 381mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Western Cape"]
[199,"RT74-02-008","Group Series 5","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Eastern Cape"]
[200,"RT74-02-008","Group Series 5","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Free State"]
[201,"RT74-02-008","Group Series 5","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Gauteng"]
[202,"RT74-02-008","Group Series 5","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Kwazulu-Natal"]
[203,"RT74-02-008","Group Series 5","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Limpopo"]
[204,"RT74-02-008","Group Series 5","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Mpumalanga"]
[205,"RT74-02-008","Group Series 5","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Northern Cape"]
[206,"RT74-02-008","Group Series 5","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","North West"]
[207,"RT74-02-008","Group Series 5","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Western Cape"]
[208,"RT74-02-009","Group Series 5","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING.\n Size 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Eastern Cape"]
[209,"RT74-02-009","Group Series 5","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING.\n Size 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Free State"]
[210,"RT74-02-009","Group Series 5","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING.\n Size 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Gauteng"]
[211,"RT74-02-009","Group Series 5","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING.\n Size 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Kwazulu-Natal"]
[212,"RT74-02-009","Group Series 5","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING.\n Size 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Limpopo"]
[213,"RT74-02-009","Group Series 5","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING.\n Size 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Mpumalanga"]
[214,"RT74-02-009","Group Series 5","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING.\n Size 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Northern Cape"]
[215,"RT74-02-009","Group Series 5","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING.\n Size 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","North West"]
[216,"RT74-02-009","Group Series 5","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING.\n Size 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Western Cape"]
[217,"RT74-02-010","Group Series 5","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS.\nSize 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Eastern Cape"]
[218,"RT74-02-010","Group Series 5","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS.\nSize 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Free State"]
[219,"RT74-02-010","Group Series 5","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS.\nSize 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Gauteng"]
[220,"RT74-02-010","Group Series 5","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS.\nSize 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Kwazulu-Natal"]
[221,"RT74-02-010","Group Series 5","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS.\nSize 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Limpopo"]
[222,"RT74-02-010","Group Series 5","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS.\nSize 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Mpumalanga"]
[223,"RT74-02-010","Group Series 5","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS.\nSize 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Northern Cape"]
[224,"RT74-02-010","Group Series 5","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS.\nSize 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","North West"]
[225,"RT74-02-010","Group Series 5","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS.\nSize 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Western Cape"]
[226,"RT74-02-011","Group Series 6","Beaded Type Shelving","ADDITIONAL SHELF FOR BEADED TYPE SHELVING UNIT\nSize 914mm wide x 457mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items :\nRT74-02-012,RT74-02-013,RT74-02-014,RT74-02-015","Eastern Cape"]
[227,"RT74-02-011","Group Series 6","Beaded Type Shelving","ADDITIONAL SHELF FOR BEADED TYPE SHELVING UNIT\nSize 914mm wide x 457mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items :\nRT74-02-012,RT74-02-013,RT74-02-014,RT74-02-015","Free State"]
[228,"RT74-02-011","Group Series 6","Beaded Type Shelving","ADDITIONAL SHELF FOR BEADED TYPE SHELVING UNIT\nSize 914mm wide x 457mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items :\nRT74-02-012,RT74-02-013,RT74-02-014,RT74-02-015","Gauteng"]
[229,"RT74-02-011","Group Series 6","Beaded Type Shelving","ADDITIONAL SHELF FOR BEADED TYPE SHELVING UNIT\nSize 914mm wide x 457mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items :\nRT74-02-012,RT74-02-013,RT74-02-014,RT74-02-015","Kwazulu-Natal"]
[230,"RT74-02-011","Group Series 6","Beaded Type Shelving","ADDITIONAL SHELF FOR BEADED TYPE SHELVING UNIT\nSize 914mm wide x 457mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items :\nRT74-02-012,RT74-02-013,RT74-02-014,RT74-02-015","Limpopo"]
[231,"RT74-02-011","Group Series 6","Beaded Type Shelving","ADDITIONAL SHELF FOR BEADED TYPE SHELVING UNIT\nSize 914mm wide x 457mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items :\nRT74-02-012,RT74-02-013,RT74-02-014,RT74-02-015","Mpumalanga"]
[232,"RT74-02-011","Group Series 6","Beaded Type Shelving","ADDITIONAL SHELF FOR BEADED TYPE SHELVING UNIT\nSize 914mm wide x 457mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items :\nRT74-02-012,RT74-02-013,RT74-02-014,RT74-02-015","Northern Cape"]
[233,"RT74-02-011","Group Series 6","Beaded Type Shelving","ADDITIONAL SHELF FOR BEADED TYPE SHELVING UNIT\nSize 914mm wide x 457mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items :\nRT74-02-012,RT74-02-013,RT74-02-014,RT74-02-015","North West"]
[234,"RT74-02-011","Group Series 6","Beaded Type Shelving","ADDITIONAL SHELF FOR BEADED TYPE SHELVING UNIT\nSize 914mm wide x 457mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items :\nRT74-02-012,RT74-02-013,RT74-02-014,RT74-02-015","Western Cape"]
[235,"RT74-02-012","Group Series 6","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Eastern Cape"]
[236,"RT74-02-012","Group Series 6","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Free State"]
[237,"RT74-02-012","Group Series 6","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Gauteng"]
[238,"RT74-02-012","Group Series 6","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Kwazulu-Natal"]
[239,"RT74-02-012","Group Series 6","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Limpopo"]
[240,"RT74-02-012","Group Series 6","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Mpumalanga"]
[241,"RT74-02-012","Group Series 6","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Northern Cape"]
[242,"RT74-02-012","Group Series 6","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","North West"]
[243,"RT74-02-012","Group Series 6","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Western Cape"]
[244,"RT74-02-013","Group Series 6","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Eastern Cape"]
[245,"RT74-02-013","Group Series 6","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Free State"]
[246,"RT74-02-013","Group Series 6","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Gauteng"]
[247,"RT74-02-013","Group Series 6","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Kwazulu-Natal"]
[248,"RT74-02-013","Group Series 6","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Limpopo"]
[249,"RT74-02-013","Group Series 6","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Mpumalanga"]
[250,"RT74-02-013","Group Series 6","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Northern Cape"]
[251,"RT74-02-013","Group Series 6","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","North West"]
[252,"RT74-02-013","Group Series 6","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Western Cape"]
[253,"RT74-02-014","Group Series 6","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 2210mm high x 914mm wide x 457mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Eastern Cape"]
[254,"RT74-02-014","Group Series 6","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 2210mm high x 914mm wide x 457mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Free State"]
[255,"RT74-02-014","Group Series 6","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 2210mm high x 914mm wide x 457mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Gauteng"]
[256,"RT74-02-014","Group Series 6","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 2210mm high x 914mm wide x 457mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Kwazulu-Natal"]
[257,"RT74-02-014","Group Series 6","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 2210mm high x 914mm wide x 457mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Limpopo"]
[258,"RT74-02-014","Group Series 6","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 2210mm high x 914mm wide x 457mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Mpumalanga"]
[259,"RT74-02-014","Group Series 6","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 2210mm high x 914mm wide x 457mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Northern Cape"]
[260,"RT74-02-014","Group Series 6","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 2210mm high x 914mm wide x 457mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","North West"]
[261,"RT74-02-014","Group Series 6","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 2210mm high x 914mm wide x 457mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Western Cape"]
[262,"RT74-02-015","Group Series 6","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 2210mm high x 914mm wide x 457mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Eastern Cape"]
[263,"RT74-02-015","Group Series 6","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 2210mm high x 914mm wide x 457mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Free State"]
[264,"RT74-02-015","Group Series 6","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 2210mm high x 914mm wide x 457mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Gauteng"]
[265,"RT74-02-015","Group Series 6","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 2210mm high x 914mm wide x 457mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Kwazulu-Natal"]
[266,"RT74-02-015","Group Series 6","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 2210mm high x 914mm wide x 457mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Limpopo"]
[267,"RT74-02-015","Group Series 6","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 2210mm high x 914mm wide x 457mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Mpumalanga"]
[268,"RT74-02-015","Group Series 6","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 2210mm high x 914mm wide x 457mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Northern Cape"]
[269,"RT74-02-015","Group Series 6","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 2210mm high x 914mm wide x 457mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","North West"]
[270,"RT74-02-015","Group Series 6","Beaded Type Shelving","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 2210mm high x 914mm wide x 457mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Western Cape"]
[271,"RT74-03-001","Group Series 7","Bolted Shelving","ADDITIONAL SHELF FOR BOLTED TYPE SHELVING UNIT. \nSize 914mm wide x 305mm deep. 1mm thick cold rolled commercial quality steel.\nTo comply with CKS 370 standard\nThis item is additional to the below items:\nRT74-03-002,RT74-03-003,RT74-03-004,RT74-03-005","Eastern Cape"]
[272,"RT74-03-001","Group Series 7","Bolted Shelving","ADDITIONAL SHELF FOR BOLTED TYPE SHELVING UNIT. \nSize 914mm wide x 305mm deep. 1mm thick cold rolled commercial quality steel.\nTo comply with CKS 370 standard\nThis item is additional to the below items:\nRT74-03-002,RT74-03-003,RT74-03-004,RT74-03-005","Free State"]
[273,"RT74-03-001","Group Series 7","Bolted Shelving","ADDITIONAL SHELF FOR BOLTED TYPE SHELVING UNIT. \nSize 914mm wide x 305mm deep. 1mm thick cold rolled commercial quality steel.\nTo comply with CKS 370 standard\nThis item is additional to the below items:\nRT74-03-002,RT74-03-003,RT74-03-004,RT74-03-005","Gauteng"]
[274,"RT74-03-001","Group Series 7","Bolted Shelving","ADDITIONAL SHELF FOR BOLTED TYPE SHELVING UNIT. \nSize 914mm wide x 305mm deep. 1mm thick cold rolled commercial quality steel.\nTo comply with CKS 370 standard\nThis item is additional to the below items:\nRT74-03-002,RT74-03-003,RT74-03-004,RT74-03-005","Kwazulu-Natal"]
[275,"RT74-03-001","Group Series 7","Bolted Shelving","ADDITIONAL SHELF FOR BOLTED TYPE SHELVING UNIT. \nSize 914mm wide x 305mm deep. 1mm thick cold rolled commercial quality steel.\nTo comply with CKS 370 standard\nThis item is additional to the below items:\nRT74-03-002,RT74-03-003,RT74-03-004,RT74-03-005","Limpopo"]
[276,"RT74-03-001","Group Series 7","Bolted Shelving","ADDITIONAL SHELF FOR BOLTED TYPE SHELVING UNIT. \nSize 914mm wide x 305mm deep. 1mm thick cold rolled commercial quality steel.\nTo comply with CKS 370 standard\nThis item is additional to the below items:\nRT74-03-002,RT74-03-003,RT74-03-004,RT74-03-005","Mpumalanga"]
[277,"RT74-03-001","Group Series 7","Bolted Shelving","ADDITIONAL SHELF FOR BOLTED TYPE SHELVING UNIT. \nSize 914mm wide x 305mm deep. 1mm thick cold rolled commercial quality steel.\nTo comply with CKS 370 standard\nThis item is additional to the below items:\nRT74-03-002,RT74-03-003,RT74-03-004,RT74-03-005","Northern Cape"]
[278,"RT74-03-001","Group Series 7","Bolted Shelving","ADDITIONAL SHELF FOR BOLTED TYPE SHELVING UNIT. \nSize 914mm wide x 305mm deep. 1mm thick cold rolled commercial quality steel.\nTo comply with CKS 370 standard\nThis item is additional to the below items:\nRT74-03-002,RT74-03-003,RT74-03-004,RT74-03-005","North West"]
[279,"RT74-03-001","Group Series 7","Bolted Shelving","ADDITIONAL SHELF FOR BOLTED TYPE SHELVING UNIT. \nSize 914mm wide x 305mm deep. 1mm thick cold rolled commercial quality steel.\nTo comply with CKS 370 standard\nThis item is additional to the below items:\nRT74-03-002,RT74-03-003,RT74-03-004,RT74-03-005","Western Cape"]
[280,"RT74-03-002","Group Series 7","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Eastern Cape"]
[281,"RT74-03-002","Group Series 7","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Free State"]
[282,"RT74-03-002","Group Series 7","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Gauteng"]
[283,"RT74-03-002","Group Series 7","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Kwazulu-Natal"]
[284,"RT74-03-002","Group Series 7","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Limpopo"]
[285,"RT74-03-002","Group Series 7","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Mpumalanga"]
[286,"RT74-03-002","Group Series 7","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Northern Cape"]
[287,"RT74-03-002","Group Series 7","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","North West"]
[288,"RT74-03-002","Group Series 7","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Western Cape"]
[289,"RT74-03-003","Group Series 7","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS. \nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Eastern Cape"]
[290,"RT74-03-003","Group Series 7","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS. \nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Free State"]
[291,"RT74-03-003","Group Series 7","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS. \nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Gauteng"]
[292,"RT74-03-003","Group Series 7","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS. \nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Kwazulu-Natal"]
[293,"RT74-03-003","Group Series 7","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS. \nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Limpopo"]
[294,"RT74-03-003","Group Series 7","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS. \nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Mpumalanga"]
[295,"RT74-03-003","Group Series 7","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS. \nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Northern Cape"]
[296,"RT74-03-003","Group Series 7","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS. \nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","North West"]
[297,"RT74-03-003","Group Series 7","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS. \nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Western Cape"]
[298,"RT74-03-004","Group Series 7","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING.\nSize 2210mm high x 914mm wide x 305mm deep. 7 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nTe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Eastern Cape"]
[299,"RT74-03-004","Group Series 7","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING.\nSize 2210mm high x 914mm wide x 305mm deep. 7 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nTe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Free State"]
[300,"RT74-03-004","Group Series 7","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING.\nSize 2210mm high x 914mm wide x 305mm deep. 7 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nTe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Gauteng"]
[301,"RT74-03-004","Group Series 7","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING.\nSize 2210mm high x 914mm wide x 305mm deep. 7 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nTe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Kwazulu-Natal"]
[302,"RT74-03-004","Group Series 7","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING.\nSize 2210mm high x 914mm wide x 305mm deep. 7 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nTe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Limpopo"]
[303,"RT74-03-004","Group Series 7","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING.\nSize 2210mm high x 914mm wide x 305mm deep. 7 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nTe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Mpumalanga"]
[304,"RT74-03-004","Group Series 7","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING.\nSize 2210mm high x 914mm wide x 305mm deep. 7 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nTe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Northern Cape"]
[305,"RT74-03-004","Group Series 7","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING.\nSize 2210mm high x 914mm wide x 305mm deep. 7 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nTe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","North West"]
[306,"RT74-03-004","Group Series 7","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING.\nSize 2210mm high x 914mm wide x 305mm deep. 7 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nTe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Western Cape"]
[307,"RT74-03-005","Group Series 7","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 2210mm high x 914mm wide x 305mm deep. 7 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Eastern Cape"]
[308,"RT74-03-005","Group Series 7","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 2210mm high x 914mm wide x 305mm deep. 7 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Free State"]
[309,"RT74-03-005","Group Series 7","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 2210mm high x 914mm wide x 305mm deep. 7 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Gauteng"]
[310,"RT74-03-005","Group Series 7","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 2210mm high x 914mm wide x 305mm deep. 7 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Kwazulu-Natal"]
[311,"RT74-03-005","Group Series 7","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 2210mm high x 914mm wide x 305mm deep. 7 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Limpopo"]
[312,"RT74-03-005","Group Series 7","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 2210mm high x 914mm wide x 305mm deep. 7 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Mpumalanga"]
[313,"RT74-03-005","Group Series 7","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 2210mm high x 914mm wide x 305mm deep. 7 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Northern Cape"]
[314,"RT74-03-005","Group Series 7","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 2210mm high x 914mm wide x 305mm deep. 7 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","North West"]
[315,"RT74-03-005","Group Series 7","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 2210mm high x 914mm wide x 305mm deep. 7 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Western Cape"]
[316,"RT74-03-006","Group Series 8","Bolted Shelving","ADDITIONAL SHELF FOR BOLTED TYPE SHELVING UNIT.\nSize 914mm wide x 381mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items: \nRT74-03-007,RT74-03-008,RT74-03-009,RT74-03-010","Eastern Cape"]
[317,"RT74-03-006","Group Series 8","Bolted Shelving","ADDITIONAL SHELF FOR BOLTED TYPE SHELVING UNIT.\nSize 914mm wide x 381mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items: \nRT74-03-007,RT74-03-008,RT74-03-009,RT74-03-010","Free State"]
[318,"RT74-03-006","Group Series 8","Bolted Shelving","ADDITIONAL SHELF FOR BOLTED TYPE SHELVING UNIT.\nSize 914mm wide x 381mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items: \nRT74-03-007,RT74-03-008,RT74-03-009,RT74-03-010","Gauteng"]
[319,"RT74-03-006","Group Series 8","Bolted Shelving","ADDITIONAL SHELF FOR BOLTED TYPE SHELVING UNIT.\nSize 914mm wide x 381mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items: \nRT74-03-007,RT74-03-008,RT74-03-009,RT74-03-010","Kwazulu-Natal"]
[320,"RT74-03-006","Group Series 8","Bolted Shelving","ADDITIONAL SHELF FOR BOLTED TYPE SHELVING UNIT.\nSize 914mm wide x 381mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items: \nRT74-03-007,RT74-03-008,RT74-03-009,RT74-03-010","Limpopo"]
[321,"RT74-03-006","Group Series 8","Bolted Shelving","ADDITIONAL SHELF FOR BOLTED TYPE SHELVING UNIT.\nSize 914mm wide x 381mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items: \nRT74-03-007,RT74-03-008,RT74-03-009,RT74-03-010","Mpumalanga"]
[322,"RT74-03-006","Group Series 8","Bolted Shelving","ADDITIONAL SHELF FOR BOLTED TYPE SHELVING UNIT.\nSize 914mm wide x 381mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items: \nRT74-03-007,RT74-03-008,RT74-03-009,RT74-03-010","Northern Cape"]
[323,"RT74-03-006","Group Series 8","Bolted Shelving","ADDITIONAL SHELF FOR BOLTED TYPE SHELVING UNIT.\nSize 914mm wide x 381mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items: \nRT74-03-007,RT74-03-008,RT74-03-009,RT74-03-010","North West"]
[324,"RT74-03-006","Group Series 8","Bolted Shelving","ADDITIONAL SHELF FOR BOLTED TYPE SHELVING UNIT.\nSize 914mm wide x 381mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items: \nRT74-03-007,RT74-03-008,RT74-03-009,RT74-03-010","Western Cape"]
[325,"RT74-03-007","Group Series 8","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 1905mm high x 914mm wide x 381mm deep. 6 x shelves including top and bottom 1mm thick colled rolled commercial quality stee\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standardd","Eastern Cape"]
[326,"RT74-03-007","Group Series 8","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 1905mm high x 914mm wide x 381mm deep. 6 x shelves including top and bottom 1mm thick colled rolled commercial quality stee\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Free State"]
[327,"RT74-03-007","Group Series 8","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 1905mm high x 914mm wide x 381mm deep. 6 x shelves including top and bottom 1mm thick colled rolled commercial quality stee\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Gauteng"]
[328,"RT74-03-007","Group Series 8","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 1905mm high x 914mm wide x 381mm deep. 6 x shelves including top and bottom 1mm thick colled rolled commercial quality stee\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Kwazulu-Natal"]
[329,"RT74-03-007","Group Series 8","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 1905mm high x 914mm wide x 381mm deep. 6 x shelves including top and bottom 1mm thick colled rolled commercial quality stee\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Limpopo"]
[330,"RT74-03-007","Group Series 8","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 1905mm high x 914mm wide x 381mm deep. 6 x shelves including top and bottom 1mm thick colled rolled commercial quality stee\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Mpumalanga"]
[331,"RT74-03-007","Group Series 8","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 1905mm high x 914mm wide x 381mm deep. 6 x shelves including top and bottom 1mm thick colled rolled commercial quality stee\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Northern Cape"]
[332,"RT74-03-007","Group Series 8","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 1905mm high x 914mm wide x 381mm deep. 6 x shelves including top and bottom 1mm thick colled rolled commercial quality stee\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","North West"]
[333,"RT74-03-007","Group Series 8","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 1905mm high x 914mm wide x 381mm deep. 6 x shelves including top and bottom 1mm thick colled rolled commercial quality stee\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Western Cape"]
[334,"RT74-03-008","Group Series 8","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom\n1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Eastern Cape"]
[335,"RT74-03-008","Group Series 8","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom\n1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Free State"]
[336,"RT74-03-008","Group Series 8","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom\n1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Gauteng"]
[337,"RT74-03-008","Group Series 8","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom\n1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Kwazulu-Natal"]
[338,"RT74-03-008","Group Series 8","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom\n1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Limpopo"]
[339,"RT74-03-008","Group Series 8","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom\n1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Mpumalanga"]
[340,"RT74-03-008","Group Series 8","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom\n1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Northern Cape"]
[341,"RT74-03-008","Group Series 8","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom\n1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","North West"]
[342,"RT74-03-008","Group Series 8","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 305mm deep. 6 x shelves including top and bottom\n1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Western Cape"]
[343,"RT74-03-009","Group Series 8","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING. \nSize 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom\n1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Eastern Cape"]
[344,"RT74-03-009","Group Series 8","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING. \nSize 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom\n1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Free State"]
[345,"RT74-03-009","Group Series 8","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING. \nSize 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom\n1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Gauteng"]
[346,"RT74-03-009","Group Series 8","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING. \nSize 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom\n1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Kwazulu-Natal"]
[347,"RT74-03-009","Group Series 8","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING. \nSize 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom\n1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Limpopo"]
[348,"RT74-03-009","Group Series 8","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING. \nSize 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom\n1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Mpumalanga"]
[349,"RT74-03-009","Group Series 8","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING. \nSize 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom\n1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Northern Cape"]
[350,"RT74-03-009","Group Series 8","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING. \nSize 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom\n1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","North West"]
[351,"RT74-03-009","Group Series 8","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING. \nSize 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom\n1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Western Cape"]
[352,"RT74-03-010","Group Series 8","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Eastern Cape"]
[353,"RT74-03-010","Group Series 8","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Free State"]
[354,"RT74-03-010","Group Series 8","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Gauteng"]
[355,"RT74-03-010","Group Series 8","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Kwazulu-Natal"]
[356,"RT74-03-010","Group Series 8","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Limpopo"]
[357,"RT74-03-010","Group Series 8","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Mpumalanga"]
[358,"RT74-03-010","Group Series 8","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Northern Cape"]
[359,"RT74-03-010","Group Series 8","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","North West"]
[360,"RT74-03-010","Group Series 8","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 2210mm high x 914mm wide x 381mm deep. 7 x shelves including top and bottom 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Western Cape"]
[361,"RT74-03-011","Group Series 9","Bolted Shelving","ADDITIONAL SHELF FOR BOLTED TYPE SHELVING UNIT.\nSize 914mm wide x 457mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items : \nRT74-03-012,RT74-03-013,RT74-03-014,RT74-03-015","Eastern Cape"]
[362,"RT74-03-011","Group Series 9","Bolted Shelving","ADDITIONAL SHELF FOR BOLTED TYPE SHELVING UNIT.\nSize 914mm wide x 457mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items : \nRT74-03-012,RT74-03-013,RT74-03-014,RT74-03-015","Free State"]
[363,"RT74-03-011","Group Series 9","Bolted Shelving","ADDITIONAL SHELF FOR BOLTED TYPE SHELVING UNIT.\nSize 914mm wide x 457mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items : \nRT74-03-012,RT74-03-013,RT74-03-014,RT74-03-015","Gauteng"]
[364,"RT74-03-011","Group Series 9","Bolted Shelving","ADDITIONAL SHELF FOR BOLTED TYPE SHELVING UNIT.\nSize 914mm wide x 457mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items : \nRT74-03-012,RT74-03-013,RT74-03-014,RT74-03-015","Kwazulu-Natal"]
[365,"RT74-03-011","Group Series 9","Bolted Shelving","ADDITIONAL SHELF FOR BOLTED TYPE SHELVING UNIT.\nSize 914mm wide x 457mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items : \nRT74-03-012,RT74-03-013,RT74-03-014,RT74-03-015","Limpopo"]
[366,"RT74-03-011","Group Series 9","Bolted Shelving","ADDITIONAL SHELF FOR BOLTED TYPE SHELVING UNIT.\nSize 914mm wide x 457mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items : \nRT74-03-012,RT74-03-013,RT74-03-014,RT74-03-015","Mpumalanga"]
[367,"RT74-03-011","Group Series 9","Bolted Shelving","ADDITIONAL SHELF FOR BOLTED TYPE SHELVING UNIT.\nSize 914mm wide x 457mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items : \nRT74-03-012,RT74-03-013,RT74-03-014,RT74-03-015","Northern Cape"]
[368,"RT74-03-011","Group Series 9","Bolted Shelving","ADDITIONAL SHELF FOR BOLTED TYPE SHELVING UNIT.\nSize 914mm wide x 457mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items : \nRT74-03-012,RT74-03-013,RT74-03-014,RT74-03-015","North West"]
[369,"RT74-03-011","Group Series 9","Bolted Shelving","ADDITIONAL SHELF FOR BOLTED TYPE SHELVING UNIT.\nSize 914mm wide x 457mm deep. 1mm thick cold rolled commercial quality steel\nTo comply with CKS 370 standard\nThis item is additional to the below items : \nRT74-03-012,RT74-03-013,RT74-03-014,","Western Cape"]
[370,"RT74-03-012","Group Series 9","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING. \nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom 1mm thick colled rolled commercial quality steel.\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Eastern Cape"]
[371,"RT74-03-012","Group Series 9","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING. \nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom 1mm thick colled rolled commercial quality steel.\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Free State"]
[372,"RT74-03-012","Group Series 9","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING. \nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom 1mm thick colled rolled commercial quality steel.\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Gauteng"]
[373,"RT74-03-012","Group Series 9","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING. \nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom 1mm thick colled rolled commercial quality steel.\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Kwazulu-Natal"]
[374,"RT74-03-012","Group Series 9","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING. \nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom 1mm thick colled rolled commercial quality steel.\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Limpopo"]
[375,"RT74-03-012","Group Series 9","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING. \nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom 1mm thick colled rolled commercial quality steel.\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Mpumalanga"]
[376,"RT74-03-012","Group Series 9","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING. \nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom 1mm thick colled rolled commercial quality steel.\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Northern Cape"]
[377,"RT74-03-012","Group Series 9","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING. \nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom 1mm thick colled rolled commercial quality steel.\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","North West"]
[378,"RT74-03-012","Group Series 9","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING. \nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom 1mm thick colled rolled commercial quality steel.\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Western Cape"]
[379,"RT74-03-013","Group Series 9","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Eastern Cape"]
[380,"RT74-03-013","Group Series 9","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Free State"]
[381,"RT74-03-013","Group Series 9","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Gauteng"]
[382,"RT74-03-013","Group Series 9","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Kwazulu-Natal"]
[383,"RT74-03-013","Group Series 9","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Limpopo"]
[384,"RT74-03-013","Group Series 9","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Mpumalanga"]
[385,"RT74-03-013","Group Series 9","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Northern Cape"]
[386,"RT74-03-013","Group Series 9","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","North West"]
[387,"RT74-03-013","Group Series 9","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSize 1905mm high x 914mm wide x 457mm deep. 6 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Western Cape"]
[388,"RT74-03-014","Group Series 9","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 2210mm high x 914mm wide x 457mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Eastern Cape"]
[389,"RT74-03-014","Group Series 9","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 2210mm high x 914mm wide x 457mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Free State"]
[390,"RT74-03-014","Group Series 9","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 2210mm high x 914mm wide x 457mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Gauteng"]
[391,"RT74-03-014","Group Series 9","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 2210mm high x 914mm wide x 457mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Kwazulu-Natal"]
[392,"RT74-03-014","Group Series 9","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 2210mm high x 914mm wide x 457mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Limpopo"]
[393,"RT74-03-014","Group Series 9","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 2210mm high x 914mm wide x 457mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Mpumalanga"]
[394,"RT74-03-014","Group Series 9","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 2210mm high x 914mm wide x 457mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Northern Cape"]
[395,"RT74-03-014","Group Series 9","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 2210mm high x 914mm wide x 457mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","North West"]
[396,"RT74-03-014","Group Series 9","Bolted Shelving","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING\nSize 2210mm high x 914mm wide x 457mm deep. 7 x shelves including top and bottom. 1mm thick colled rolled commercial quality steel\nUniformly distributed mass load of 170kg per shelf\nThe unit must be fully adjustable to allow for additional shelves\nTo comply with CKS 370 standard","Western Cape"]
[397,"RT74-04-001","Not Applicable","Heavy Duty Steel Racking","HEAVY DUTY STEEL RACKING WITH NO DECKING\nSize 3353mm high x 2743mm wide x 900mm deep. 4 x beam levels to the height Uniformly distributed load of 3000kg per beam level\nUnit must be fully ajustable to allow for additional beam levels to be added\n","Eastern Cape"]
[398,"RT74-04-001","Not Applicable","Heavy Duty Steel Racking","HEAVY DUTY STEEL RACKING WITH NO DECKING\nSize 3353mm high x 2743mm wide x 900mm deep. 4 x beam levels to the height Uniformly distributed load of 3000kg per beam level\nUnit must be fully ajustable to allow for additional beam levels to be added\n","Free State"]
[399,"RT74-04-001","Not Applicable","Heavy Duty Steel Racking","HEAVY DUTY STEEL RACKING WITH NO DECKING\nSize 3353mm high x 2743mm wide x 900mm deep. 4 x beam levels to the height Uniformly distributed load of 3000kg per beam level\nUnit must be fully ajustable to allow for additional beam levels to be added\n","Gauteng"]
[400,"RT74-04-001","Not Applicable","Heavy Duty Steel Racking","HEAVY DUTY STEEL RACKING WITH NO DECKING\nSize 3353mm high x 2743mm wide x 900mm deep. 4 x beam levels to the height Uniformly distributed load of 3000kg per beam level\nUnit must be fully ajustable to allow for additional beam levels to be added\n","Kwazulu-Natal"]
[401,"RT74-04-001","Not Applicable","Heavy Duty Steel Racking","HEAVY DUTY STEEL RACKING WITH NO DECKING\nSize 3353mm high x 2743mm wide x 900mm deep. 4 x beam levels to the height Uniformly distributed load of 3000kg per beam level\nUnit must be fully ajustable to allow for additional beam levels to be added\n","Limpopo"]
[402,"RT74-04-001","Not Applicable","Heavy Duty Steel Racking","HEAVY DUTY STEEL RACKING WITH NO DECKING\nSize 3353mm high x 2743mm wide x 900mm deep. 4 x beam levels to the height Uniformly distributed load of 3000kg per beam level\nUnit must be fully ajustable to allow for additional beam levels to be added\n","Mpumalanga"]
[403,"RT74-04-001","Not Applicable","Heavy Duty Steel Racking","HEAVY DUTY STEEL RACKING WITH NO DECKING\nSize 3353mm high x 2743mm wide x 900mm deep. 4 x beam levels to the height Uniformly distributed load of 3000kg per beam level\nUnit must be fully ajustable to allow for additional beam levels to be added\n","Northern Cape"]
[404,"RT74-04-001","Not Applicable","Heavy Duty Steel Racking","HEAVY DUTY STEEL RACKING WITH NO DECKING\nSize 3353mm high x 2743mm wide x 900mm deep. 4 x beam levels to the height Uniformly distributed load of 3000kg per beam level\nUnit must be fully ajustable to allow for additional beam levels to be added\n","North West"]
[405,"RT74-04-001","Not Applicable","Heavy Duty Steel Racking","HEAVY DUTY STEEL RACKING WITH NO DECKING\nSize 3353mm high x 2743mm wide x 900mm deep. 4 x beam levels to the height Uniformly distributed load of 3000kg per beam level\nUnit must be fully ajustable to allow for additional beam levels to be added\n","Western Cape"]
[406,"RT74-04-002","Not Applicable","Heavy Duty Steel Racking","HEAVY DUTY STEEL RACKING WITH TIMBER DECKING.\nSize 3353mm high x 2743mm wide x 900mm deep. 4 x beam levels to the height\n25mm thick timber decking\nUniformly distributed load of 3000kg per beam level\nUnit must be fully adjustable to allow for additional beam levels to be added\n","Eastern Cape"]
[407,"RT74-04-002","Not Applicable","Heavy Duty Steel Racking","HEAVY DUTY STEEL RACKING WITH TIMBER DECKING.\nSize 3353mm high x 2743mm wide x 900mm deep. 4 x beam levels to the height\n25mm thick timber decking\nUniformly distributed load of 3000kg per beam level\nUnit must be fully adjustable to allow for additional beam levels to be added\n","Free State"]
[408,"RT74-04-002","Not Applicable","Heavy Duty Steel Racking","HEAVY DUTY STEEL RACKING WITH TIMBER DECKING.\nSize 3353mm high x 2743mm wide x 900mm deep. 4 x beam levels to the height\n25mm thick timber decking\nUniformly distributed load of 3000kg per beam level\nUnit must be fully adjustable to allow for additional beam levels to be added\n","Gauteng"]
[409,"RT74-04-002","Not Applicable","Heavy Duty Steel Racking","HEAVY DUTY STEEL RACKING WITH TIMBER DECKING.\nSize 3353mm high x 2743mm wide x 900mm deep. 4 x beam levels to the height\n25mm thick timber decking\nUniformly distributed load of 3000kg per beam level\nUnit must be fully adjustable to allow for additional beam levels to be added\n","Kwazulu-Natal"]
[410,"RT74-04-002","Not Applicable","Heavy Duty Steel Racking","HEAVY DUTY STEEL RACKING WITH TIMBER DECKING.\nSize 3353mm high x 2743mm wide x 900mm deep. 4 x beam levels to the height\n25mm thick timber decking\nUniformly distributed load of 3000kg per beam level\nUnit must be fully adjustable to allow for additional beam levels to be added\n","Limpopo"]
[411,"RT74-04-002","Not Applicable","Heavy Duty Steel Racking","HEAVY DUTY STEEL RACKING WITH TIMBER DECKING.\nSize 3353mm high x 2743mm wide x 900mm deep. 4 x beam levels to the height\n25mm thick timber decking\nUniformly distributed load of 3000kg per beam level\nUnit must be fully adjustable to allow for additional beam levels to be added\n","Mpumalanga"]
[412,"RT74-04-002","Not Applicable","Heavy Duty Steel Racking","HEAVY DUTY STEEL RACKING WITH TIMBER DECKING.\nSize 3353mm high x 2743mm wide x 900mm deep. 4 x beam levels to the height\n25mm thick timber decking\nUniformly distributed load of 3000kg per beam level\nUnit must be fully adjustable to allow for additional beam levels to be added\n","Northern Cape"]
[413,"RT74-04-002","Not Applicable","Heavy Duty Steel Racking","HEAVY DUTY STEEL RACKING WITH TIMBER DECKING.\nSize 3353mm high x 2743mm wide x 900mm deep. 4 x beam levels to the height\n25mm thick timber decking\nUniformly distributed load of 3000kg per beam level\nUnit must be fully adjustable to allow for additional beam levels to be added\n","North West"]
[414,"RT74-04-002","Not Applicable","Heavy Duty Steel Racking","HEAVY DUTY STEEL RACKING WITH TIMBER DECKING.\nSize 3353mm high x 2743mm wide x 900mm deep. 4 x beam levels to the height\n25mm thick timber decking\nUniformly distributed load of 3000kg per beam level\nUnit must be fully adjustable to allow for additional beam levels to be added\n","Western Cape"]
[415,"RT74-04-003","Not Applicable","Heavy Duty Steel Racking","HEAVY DUTY STEEL RACKING WITH STEEL DECKING\nSize 3353mm high x 2743mm wide x 900mm deep. 4 x beam levels to the height\n1mm thick steel decking. uniformly distributed load of 3000kg per beam level\nUnit must be fully adjustable to allow for additional beam levels to be added\n","Eastern Cape"]
[416,"RT74-04-003","Not Applicable","Heavy Duty Steel Racking","HEAVY DUTY STEEL RACKING WITH STEEL DECKING\nSize 3353mm high x 2743mm wide x 900mm deep. 4 x beam levels to the height\n1mm thick steel decking. uniformly distributed load of 3000kg per beam level\nUnit must be fully adjustable to allow for additional beam levels to be added\n","Free State"]
[417,"RT74-04-003","Not Applicable","Heavy Duty Steel Racking","HEAVY DUTY STEEL RACKING WITH STEEL DECKING\nSize 3353mm high x 2743mm wide x 900mm deep. 4 x beam levels to the height\n1mm thick steel decking. uniformly distributed load of 3000kg per beam level\nUnit must be fully adjustable to allow for additional beam levels to be added\n","Gauteng"]
[418,"RT74-04-003","Not Applicable","Heavy Duty Steel Racking","HEAVY DUTY STEEL RACKING WITH STEEL DECKING\nSize 3353mm high x 2743mm wide x 900mm deep. 4 x beam levels to the height\n1mm thick steel decking. uniformly distributed load of 3000kg per beam level\nUnit must be fully adjustable to allow for additional beam levels to be added\n","Kwazulu-Natal"]
[419,"RT74-04-003","Not Applicable","Heavy Duty Steel Racking","HEAVY DUTY STEEL RACKING WITH STEEL DECKING\nSize 3353mm high x 2743mm wide x 900mm deep. 4 x beam levels to the height\n1mm thick steel decking. uniformly distributed load of 3000kg per beam level\nUnit must be fully adjustable to allow for additional beam levels to be added\n","Limpopo"]
[420,"RT74-04-003","Not Applicable","Heavy Duty Steel Racking","HEAVY DUTY STEEL RACKING WITH STEEL DECKING\nSize 3353mm high x 2743mm wide x 900mm deep. 4 x beam levels to the height\n1mm thick steel decking. uniformly distributed load of 3000kg per beam level\nUnit must be fully adjustable to allow for additional beam levels to be added\n","Mpumalanga"]
[421,"RT74-04-003","Not Applicable","Heavy Duty Steel Racking","HEAVY DUTY STEEL RACKING WITH STEEL DECKING\nSize 3353mm high x 2743mm wide x 900mm deep. 4 x beam levels to the height\n1mm thick steel decking. uniformly distributed load of 3000kg per beam level\nUnit must be fully adjustable to allow for additional beam levels to be added\n","Northern Cape"]
[422,"RT74-04-003","Not Applicable","Heavy Duty Steel Racking","HEAVY DUTY STEEL RACKING WITH STEEL DECKING\nSize 3353mm high x 2743mm wide x 900mm deep. 4 x beam levels to the height\n1mm thick steel decking. uniformly distributed load of 3000kg per beam level\nUnit must be fully adjustable to allow for additional beam levels to be added\n","North West"]
[423,"RT74-04-003","Not Applicable","Heavy Duty Steel Racking","HEAVY DUTY STEEL RACKING WITH STEEL DECKING\nSize 3353mm high x 2743mm wide x 900mm deep. 4 x beam levels to the height\n1mm thick steel decking. uniformly distributed load of 3000kg per beam level\nUnit must be fully adjustable to allow for additional beam levels to be added\n","Western Cape"]
[424,"RT74-04-004","Not Applicable","Heavy Duty Rack Supported Mezzanine Floor ","HEAVY DUTY RACK SUPPORTED MEZZANINE FLOOR\nCompatible with heavy duty racking placed on the floor\nUniformly distributed load of 350kg/m². floor to be covered with timber decking\nPrice includes statnchions , staircase and handrails\n","Eastern Cape"]
[425,"RT74-04-004","Not Applicable","Heavy Duty Rack Supported Mezzanine Floor ","HEAVY DUTY RACK SUPPORTED MEZZANINE FLOOR\nCompatible with heavy duty racking placed on the floor\nUniformly distributed load of 350kg/m². floor to be covered with timber decking\nPrice includes statnchions , staircase and handrails\n","Free State"]
[426,"RT74-04-004","Not Applicable","Heavy Duty Rack Supported Mezzanine Floor ","HEAVY DUTY RACK SUPPORTED MEZZANINE FLOOR\nCompatible with heavy duty racking placed on the floor\nUniformly distributed load of 350kg/m². floor to be covered with timber decking\nPrice includes statnchions , staircase and handrails\n","Gauteng"]
[427,"RT74-04-004","Not Applicable","Heavy Duty Rack Supported Mezzanine Floor ","HEAVY DUTY RACK SUPPORTED MEZZANINE FLOOR\nCompatible with heavy duty racking placed on the floor\nUniformly distributed load of 350kg/m². floor to be covered with timber decking\nPrice includes statnchions , staircase and handrails\n","Kwazulu-Natal"]
[428,"RT74-04-004","Not Applicable","Heavy Duty Rack Supported Mezzanine Floor ","HEAVY DUTY RACK SUPPORTED MEZZANINE FLOOR\nCompatible with heavy duty racking placed on the floor\nUniformly distributed load of 350kg/m². floor to be covered with timber decking\nPrice includes statnchions , staircase and handrails\n","Limpopo"]
[429,"RT74-04-004","Not Applicable","Heavy Duty Rack Supported Mezzanine Floor ","HEAVY DUTY RACK SUPPORTED MEZZANINE FLOOR\nCompatible with heavy duty racking placed on the floor\nUniformly distributed load of 350kg/m². floor to be covered with timber decking\nPrice includes statnchions , staircase and handrails\n","Mpumalanga"]
[430,"RT74-04-004","Not Applicable","Heavy Duty Rack Supported Mezzanine Floor ","HEAVY DUTY RACK SUPPORTED MEZZANINE FLOOR\nCompatible with heavy duty racking placed on the floor\nUniformly distributed load of 350kg/m². floor to be covered with timber decking\nPrice includes statnchions , staircase and handrails\n","Northern Cape"]
[431,"RT74-04-004","Not Applicable","Heavy Duty Rack Supported Mezzanine Floor ","HEAVY DUTY RACK SUPPORTED MEZZANINE FLOOR\nCompatible with heavy duty racking placed on the floor\nUniformly distributed load of 350kg/m². floor to be covered with timber decking\nPrice includes statnchions , staircase and handrails\n","North West"]
[432,"RT74-04-004","Not Applicable","Heavy Duty Rack Supported Mezzanine Floor ","HEAVY DUTY RACK SUPPORTED MEZZANINE FLOOR\nCompatible with heavy duty racking placed on the floor\nUniformly distributed load of 350kg/m². floor to be covered with timber decking\nPrice includes statnchions , staircase and handrails\n","Western Cape"]
[433,"RT74-04-005","Not Applicable","Heavy Duty Rack Supported Mezzanine Floor ","HEAVY DUTY RACK SUPPORTED MEZZANINE FLOOR. \nCompatible with heavy duty racking placed on the floor\nUniformly distributed load of 350kg/m². floor to be covered with steel decking\nPrice includes statnchions , staircase and handrails\n","Eastern Cape"]
[434,"RT74-04-005","Not Applicable","Heavy Duty Rack Supported Mezzanine Floor ","HEAVY DUTY RACK SUPPORTED MEZZANINE FLOOR. \nCompatible with heavy duty racking placed on the floor\nUniformly distributed load of 350kg/m². floor to be covered with steel decking\nPrice includes statnchions , staircase and handrails\n","Free State"]
[435,"RT74-04-005","Not Applicable","Heavy Duty Rack Supported Mezzanine Floor ","HEAVY DUTY RACK SUPPORTED MEZZANINE FLOOR. \nCompatible with heavy duty racking placed on the floor\nUniformly distributed load of 350kg/m². floor to be covered with steel decking\nPrice includes statnchions , staircase and handrails\n","Gauteng"]
[436,"RT74-04-005","Not Applicable","Heavy Duty Rack Supported Mezzanine Floor ","HEAVY DUTY RACK SUPPORTED MEZZANINE FLOOR. \nCompatible with heavy duty racking placed on the floor\nUniformly distributed load of 350kg/m². floor to be covered with steel decking\nPrice includes statnchions , staircase and handrails\n","Kwazulu-Natal"]
[437,"RT74-04-005","Not Applicable","Heavy Duty Rack Supported Mezzanine Floor ","HEAVY DUTY RACK SUPPORTED MEZZANINE FLOOR. \nCompatible with heavy duty racking placed on the floor\nUniformly distributed load of 350kg/m². floor to be covered with steel decking\nPrice includes statnchions , staircase and handrails\n","Limpopo"]
[438,"RT74-04-005","Not Applicable","Heavy Duty Rack Supported Mezzanine Floor ","HEAVY DUTY RACK SUPPORTED MEZZANINE FLOOR. \nCompatible with heavy duty racking placed on the floor\nUniformly distributed load of 350kg/m². floor to be covered with steel decking\nPrice includes statnchions , staircase and handrails\n","Mpumalanga"]
[439,"RT74-04-005","Not Applicable","Heavy Duty Rack Supported Mezzanine Floor ","HEAVY DUTY RACK SUPPORTED MEZZANINE FLOOR. \nCompatible with heavy duty racking placed on the floor\nUniformly distributed load of 350kg/m². floor to be covered with steel decking\nPrice includes statnchions , staircase and handrails\n","Northern Cape"]
[440,"RT74-04-005","Not Applicable","Heavy Duty Rack Supported Mezzanine Floor ","HEAVY DUTY RACK SUPPORTED MEZZANINE FLOOR. \nCompatible with heavy duty racking placed on the floor\nUniformly distributed load of 350kg/m². floor to be covered with steel decking\nPrice includes statnchions , staircase and handrails\n","North West"]
[441,"RT74-04-005","Not Applicable","Heavy Duty Rack Supported Mezzanine Floor ","HEAVY DUTY RACK SUPPORTED MEZZANINE FLOOR. \nCompatible with heavy duty racking placed on the floor\nUniformly distributed load of 350kg/m². floor to be covered with steel decking\nPrice includes statnchions , staircase and handrails\n","Western Cape"]
[442,"RT74-04-006","Not Applicable","Shelving Supported Mezzaanine Floor","SHELVING SUPPORTED MEZZANINE FLOOR (CATWALK SYSTEM).\nCompatible with shelving placed on the floor. uniformly distributed load of 350kg/m² Price includes statnchions , staircase and handrails\n","Eastern Cape"]
[443,"RT74-04-006","Not Applicable","Shelving Supported Mezzaanine Floor","SHELVING SUPPORTED MEZZANINE FLOOR (CATWALK SYSTEM).\nCompatible with shelving placed on the floor. uniformly distributed load of 350kg/m² Price includes statnchions , staircase and handrails\n","Free State"]
[444,"RT74-04-006","Not Applicable","Shelving Supported Mezzaanine Floor","SHELVING SUPPORTED MEZZANINE FLOOR (CATWALK SYSTEM).\nCompatible with shelving placed on the floor. uniformly distributed load of 350kg/m² Price includes statnchions , staircase and handrails\n","Gauteng"]
[445,"RT74-04-006","Not Applicable","Shelving Supported Mezzaanine Floor","SHELVING SUPPORTED MEZZANINE FLOOR (CATWALK SYSTEM).\nCompatible with shelving placed on the floor. uniformly distributed load of 350kg/m² Price includes statnchions , staircase and handrails\n","Kwazulu-Natal"]
[446,"RT74-04-006","Not Applicable","Shelving Supported Mezzaanine Floor","SHELVING SUPPORTED MEZZANINE FLOOR (CATWALK SYSTEM).\nCompatible with shelving placed on the floor. uniformly distributed load of 350kg/m² Price includes statnchions , staircase and handrails\n","Limpopo"]
[447,"RT74-04-006","Not Applicable","Shelving Supported Mezzaanine Floor","SHELVING SUPPORTED MEZZANINE FLOOR (CATWALK SYSTEM).\nCompatible with shelving placed on the floor. uniformly distributed load of 350kg/m² Price includes statnchions , staircase and handrails\n","Mpumalanga"]
[448,"RT74-04-006","Not Applicable","Shelving Supported Mezzaanine Floor","SHELVING SUPPORTED MEZZANINE FLOOR (CATWALK SYSTEM).\nCompatible with shelving placed on the floor. uniformly distributed load of 350kg/m² Price includes statnchions , staircase and handrails\n","Northern Cape"]
[449,"RT74-04-006","Not Applicable","Shelving Supported Mezzaanine Floor","SHELVING SUPPORTED MEZZANINE FLOOR (CATWALK SYSTEM).\nCompatible with shelving placed on the floor. uniformly distributed load of 350kg/m² Price includes statnchions , staircase and handrails\n","North West"]
[450,"RT74-04-006","Not Applicable","Shelving Supported Mezzaanine Floor","SHELVING SUPPORTED MEZZANINE FLOOR (CATWALK SYSTEM).\nCompatible with shelving placed on the floor. uniformly distributed load of 350kg/m² Price includes statnchions , staircase and handrails\n","Western Cape"]
[451,"RT74-04-007","Not Applicable","Structural Mezzanine Floor","STRUCTURAL MEZZANINE FLOOR.\nFree standing independent floor\nUniformly distributed load of 350kg/m². floor to be covered with steel decking\nPrice includes statnchions , staircase and handrails\n","Eastern Cape"]
[452,"RT74-04-007","Not Applicable","Structural Mezzanine Floor","STRUCTURAL MEZZANINE FLOOR.\nFree standing independent floor\nUniformly distributed load of 350kg/m². floor to be covered with steel decking\nPrice includes statnchions , staircase and handrails\n","Free State"]
[453,"RT74-04-007","Not Applicable","Structural Mezzanine Floor","STRUCTURAL MEZZANINE FLOOR.\nFree standing independent floor\nUniformly distributed load of 350kg/m². floor to be covered with steel decking\nPrice includes statnchions , staircase and handrails\n","Gauteng"]
[454,"RT74-04-007","Not Applicable","Structural Mezzanine Floor","STRUCTURAL MEZZANINE FLOOR.\nFree standing independent floor\nUniformly distributed load of 350kg/m². floor to be covered with steel decking\nPrice includes statnchions , staircase and handrails\n","Kwazulu-Natal"]
[455,"RT74-04-007","Not Applicable","Structural Mezzanine Floor","STRUCTURAL MEZZANINE FLOOR.\nFree standing independent floor\nUniformly distributed load of 350kg/m². floor to be covered with steel decking\nPrice includes statnchions , staircase and handrails\n","Limpopo"]
[456,"RT74-04-007","Not Applicable","Structural Mezzanine Floor","STRUCTURAL MEZZANINE FLOOR.\nFree standing independent floor\nUniformly distributed load of 350kg/m². floor to be covered with steel decking\nPrice includes statnchions , staircase and handrails\n","Mpumalanga"]
[457,"RT74-04-007","Not Applicable","Structural Mezzanine Floor","STRUCTURAL MEZZANINE FLOOR.\nFree standing independent floor\nUniformly distributed load of 350kg/m². floor to be covered with steel decking\nPrice includes statnchions , staircase and handrails\n","Northern Cape"]
[458,"RT74-04-007","Not Applicable","Structural Mezzanine Floor","STRUCTURAL MEZZANINE FLOOR.\nFree standing independent floor\nUniformly distributed load of 350kg/m². floor to be covered with steel decking\nPrice includes statnchions , staircase and handrails\n","North West"]
[459,"RT74-04-007","Not Applicable","Structural Mezzanine Floor","STRUCTURAL MEZZANINE FLOOR.\nFree standing independent floor\nUniformly distributed load of 350kg/m². floor to be covered with steel decking\nPrice includes statnchions , staircase and handrails\n","Western Cape"]
[460,"RT74-04-008","Not Applicable","Structural Mezzanine Floor","STRUCTURAL MEZZANINE FLOOR. \nFree standing independent floor\nUniformly distributed load of 350kg/m². floor to be covered with timber decking\nPrice includes statnchions , staircase and handrails\n","Eastern Cape"]
[461,"RT74-04-008","Not Applicable","Structural Mezzanine Floor","STRUCTURAL MEZZANINE FLOOR. \nFree standing independent floor\nUniformly distributed load of 350kg/m². floor to be covered with timber decking\nPrice includes statnchions , staircase and handrails\n","Free State"]
[462,"RT74-04-008","Not Applicable","Structural Mezzanine Floor","STRUCTURAL MEZZANINE FLOOR. \nFree standing independent floor\nUniformly distributed load of 350kg/m². floor to be covered with timber decking\nPrice includes statnchions , staircase and handrails\n","Gauteng"]
[463,"RT74-04-008","Not Applicable","Structural Mezzanine Floor","STRUCTURAL MEZZANINE FLOOR. \nFree standing independent floor\nUniformly distributed load of 350kg/m². floor to be covered with timber decking\nPrice includes statnchions , staircase and handrails\n","Kwazulu-Natal"]
[464,"RT74-04-008","Not Applicable","Structural Mezzanine Floor","STRUCTURAL MEZZANINE FLOOR. \nFree standing independent floor\nUniformly distributed load of 350kg/m². floor to be covered with timber decking\nPrice includes statnchions , staircase and handrails\n","Limpopo"]
[465,"RT74-04-008","Not Applicable","Structural Mezzanine Floor","STRUCTURAL MEZZANINE FLOOR. \nFree standing independent floor\nUniformly distributed load of 350kg/m². floor to be covered with timber decking\nPrice includes statnchions , staircase and handrails\n","Mpumalanga"]
[466,"RT74-04-008","Not Applicable","Structural Mezzanine Floor","STRUCTURAL MEZZANINE FLOOR. \nFree standing independent floor\nUniformly distributed load of 350kg/m². floor to be covered with timber decking\nPrice includes statnchions , staircase and handrails\n","Northern Cape"]
[467,"RT74-04-008","Not Applicable","Structural Mezzanine Floor","STRUCTURAL MEZZANINE FLOOR. \nFree standing independent floor\nUniformly distributed load of 350kg/m². floor to be covered with timber decking\nPrice includes statnchions , staircase and handrails\n","North West"]
[468,"RT74-04-008","Not Applicable","Structural Mezzanine Floor","STRUCTURAL MEZZANINE FLOOR. \nFree standing independent floor\nUniformly distributed load of 350kg/m². floor to be covered with timber decking\nPrice includes statnchions , staircase and handrails\n","Western Cape"]
[469,"RT74-05-001","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 01 DEEP 03 BASES (HANDLE OPERATED).\n2103mm high x 920mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Eastern Cape"]
[470,"RT74-05-001","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 01 DEEP 03 BASES (HANDLE OPERATED).\n2103mm high x 920mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Free State"]
[471,"RT74-05-001","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 01 DEEP 03 BASES (HANDLE OPERATED).\n2103mm high x 920mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Gauteng"]
[472,"RT74-05-001","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 01 DEEP 03 BASES (HANDLE OPERATED).\n2103mm high x 920mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Kwazulu-Natal"]
[473,"RT74-05-001","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 01 DEEP 03 BASES (HANDLE OPERATED).\n2103mm high x 920mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Limpopo"]
[474,"RT74-05-001","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 01 DEEP 03 BASES (HANDLE OPERATED).\n2103mm high x 920mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Mpumalanga"]
[475,"RT74-05-001","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 01 DEEP 03 BASES (HANDLE OPERATED).\n2103mm high x 920mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Northern Cape"]
[476,"RT74-05-001","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 01 DEEP 03 BASES (HANDLE OPERATED).\n2103mm high x 920mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","North West"]
[477,"RT74-05-001","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 01 DEEP 03 BASES (HANDLE OPERATED).\n2103mm high x 920mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Western Cape"]
[478,"RT74-05-002","Not Applicable","Mobile Shelving","ADDITIONAL MOBILE FILING SYSTEM 01 DEEP 01 BASE (HANDLE OPERATED).\n2103mm high x 920mm wide x 381mm deep. 6 x shelves to the height. unit has back panels and side panels. unit consists of 1 x single movable base \n","Eastern Cape"]
[479,"RT74-05-002","Not Applicable","Mobile Shelving","ADDITIONAL MOBILE FILING SYSTEM 01 DEEP 01 BASE (HANDLE OPERATED).\n2103mm high x 920mm wide x 381mm deep. 6 x shelves to the height. unit has back panels and side panels. unit consists of 1 x single movable base \n","Free State"]
[480,"RT74-05-002","Not Applicable","Mobile Shelving","ADDITIONAL MOBILE FILING SYSTEM 01 DEEP 01 BASE (HANDLE OPERATED).\n2103mm high x 920mm wide x 381mm deep. 6 x shelves to the height. unit has back panels and side panels. unit consists of 1 x single movable base \n","Gauteng"]
[481,"RT74-05-002","Not Applicable","Mobile Shelving","ADDITIONAL MOBILE FILING SYSTEM 01 DEEP 01 BASE (HANDLE OPERATED).\n2103mm high x 920mm wide x 381mm deep. 6 x shelves to the height. unit has back panels and side panels. unit consists of 1 x single movable base \n","Kwazulu-Natal"]
[482,"RT74-05-002","Not Applicable","Mobile Shelving","ADDITIONAL MOBILE FILING SYSTEM 01 DEEP 01 BASE (HANDLE OPERATED).\n2103mm high x 920mm wide x 381mm deep. 6 x shelves to the height. unit has back panels and side panels. unit consists of 1 x single movable base \n","Limpopo"]
[483,"RT74-05-002","Not Applicable","Mobile Shelving","ADDITIONAL MOBILE FILING SYSTEM 01 DEEP 01 BASE (HANDLE OPERATED).\n2103mm high x 920mm wide x 381mm deep. 6 x shelves to the height. unit has back panels and side panels. unit consists of 1 x single movable base \n","Mpumalanga"]
[484,"RT74-05-002","Not Applicable","Mobile Shelving","ADDITIONAL MOBILE FILING SYSTEM 01 DEEP 01 BASE (HANDLE OPERATED).\n2103mm high x 920mm wide x 381mm deep. 6 x shelves to the height. unit has back panels and side panels. unit consists of 1 x single movable base \n","Northern Cape"]
[485,"RT74-05-002","Not Applicable","Mobile Shelving","ADDITIONAL MOBILE FILING SYSTEM 01 DEEP 01 BASE (HANDLE OPERATED).\n2103mm high x 920mm wide x 381mm deep. 6 x shelves to the height. unit has back panels and side panels. unit consists of 1 x single movable base \n","North West"]
[486,"RT74-05-002","Not Applicable","Mobile Shelving","ADDITIONAL MOBILE FILING SYSTEM 01 DEEP 01 BASE (HANDLE OPERATED).\n2103mm high x 920mm wide x 381mm deep. 6 x shelves to the height. unit has back panels and side panels. unit consists of 1 x single movable base \n","Western Cape"]
[487,"RT74-05-003","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 02 DEEP 03 BASES (HANDLE OPERATED).\n2103mm high x 1840mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Eastern Cape"]
[488,"RT74-05-003","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 02 DEEP 03 BASES (HANDLE OPERATED).\n2103mm high x 1840mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Free State"]
[489,"RT74-05-003","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 02 DEEP 03 BASES (HANDLE OPERATED).\n2103mm high x 1840mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Gauteng"]
[490,"RT74-05-003","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 02 DEEP 03 BASES (HANDLE OPERATED).\n2103mm high x 1840mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Kwazulu-Natal"]
[491,"RT74-05-003","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 02 DEEP 03 BASES (HANDLE OPERATED).\n2103mm high x 1840mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Limpopo"]
[492,"RT74-05-003","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 02 DEEP 03 BASES (HANDLE OPERATED).\n2103mm high x 1840mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Mpumalanga"]
[493,"RT74-05-003","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 02 DEEP 03 BASES (HANDLE OPERATED).\n2103mm high x 1840mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Northern Cape"]
[494,"RT74-05-003","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 02 DEEP 03 BASES (HANDLE OPERATED).\n2103mm high x 1840mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","North West"]
[495,"RT74-05-003","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 02 DEEP 03 BASES (HANDLE OPERATED).\n2103mm high x 1840mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Western Cape"]
[496,"RT74-05-004","Not Applicable","Mobile Shelving","ADDITIONAL MOBILE FILING SYSTEM 02 DEEP 01 BASE (HANDLE OPERATED). \n2103mm high x 1840mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","Eastern Cape"]
[497,"RT74-05-004","Not Applicable","Mobile Shelving","ADDITIONAL MOBILE FILING SYSTEM 02 DEEP 01 BASE (HANDLE OPERATED). \n2103mm high x 1840mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","Free State"]
[498,"RT74-05-004","Not Applicable","Mobile Shelving","ADDITIONAL MOBILE FILING SYSTEM 02 DEEP 01 BASE (HANDLE OPERATED). \n2103mm high x 1840mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","Gauteng"]
[499,"RT74-05-004","Not Applicable","Mobile Shelving","ADDITIONAL MOBILE FILING SYSTEM 02 DEEP 01 BASE (HANDLE OPERATED). \n2103mm high x 1840mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","Kwazulu-Natal"]
[500,"RT74-05-004","Not Applicable","Mobile Shelving","ADDITIONAL MOBILE FILING SYSTEM 02 DEEP 01 BASE (HANDLE OPERATED). \n2103mm high x 1840mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","Limpopo"]
[501,"RT74-05-004","Not Applicable","Mobile Shelving","ADDITIONAL MOBILE FILING SYSTEM 02 DEEP 01 BASE (HANDLE OPERATED). \n2103mm high x 1840mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","Mpumalanga"]
[502,"RT74-05-004","Not Applicable","Mobile Shelving","ADDITIONAL MOBILE FILING SYSTEM 02 DEEP 01 BASE (HANDLE OPERATED). \n2103mm high x 1840mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","Northern Cape"]
[503,"RT74-05-004","Not Applicable","Mobile Shelving","ADDITIONAL MOBILE FILING SYSTEM 02 DEEP 01 BASE (HANDLE OPERATED). \n2103mm high x 1840mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","North West"]
[504,"RT74-05-004","Not Applicable","Mobile Shelving","ADDITIONAL MOBILE FILING SYSTEM 02 DEEP 01 BASE (HANDLE OPERATED). \n2103mm high x 1840mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","Western Cape"]
[505,"RT74-05-005","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 03 DEEP 03 BASES (STEERING WHEEL OPERATED). \n2103mm high x 2760mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Eastern Cape"]
[506,"RT74-05-005","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 03 DEEP 03 BASES (STEERING WHEEL OPERATED). \n2103mm high x 2760mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Free State"]
[507,"RT74-05-005","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 03 DEEP 03 BASES (STEERING WHEEL OPERATED). \n2103mm high x 2760mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Gauteng"]
[508,"RT74-05-005","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 03 DEEP 03 BASES (STEERING WHEEL OPERATED). \n2103mm high x 2760mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Kwazulu-Natal"]
[509,"RT74-05-005","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 03 DEEP 03 BASES (STEERING WHEEL OPERATED). \n2103mm high x 2760mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Limpopo"]
[510,"RT74-05-005","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 03 DEEP 03 BASES (STEERING WHEEL OPERATED). \n2103mm high x 2760mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Mpumalanga"]
[511,"RT74-05-005","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 03 DEEP 03 BASES (STEERING WHEEL OPERATED). \n2103mm high x 2760mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Northern Cape"]
[512,"RT74-05-005","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 03 DEEP 03 BASES (STEERING WHEEL OPERATED). \n2103mm high x 2760mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","North West"]
[513,"RT74-05-005","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 03 DEEP 03 BASES (STEERING WHEEL OPERATED). \n2103mm high x 2760mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Western Cape"]
[514,"RT74-05-006","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 03 DEEP 01 BASE (STEERING WHEEL OPERATED).\n2103mm high x 2760mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","Eastern Cape"]
[515,"RT74-05-006","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 03 DEEP 01 BASE (STEERING WHEEL OPERATED).\n2103mm high x 2760mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","Free State"]
[516,"RT74-05-006","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 03 DEEP 01 BASE (STEERING WHEEL OPERATED).\n2103mm high x 2760mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","Gauteng"]
[517,"RT74-05-006","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 03 DEEP 01 BASE (STEERING WHEEL OPERATED).\n2103mm high x 2760mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","Kwazulu-Natal"]
[518,"RT74-05-006","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 03 DEEP 01 BASE (STEERING WHEEL OPERATED).\n2103mm high x 2760mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","Limpopo"]
[519,"RT74-05-006","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 03 DEEP 01 BASE (STEERING WHEEL OPERATED).\n2103mm high x 2760mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","Mpumalanga"]
[520,"RT74-05-006","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 03 DEEP 01 BASE (STEERING WHEEL OPERATED).\n2103mm high x 2760mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","Northern Cape"]
[521,"RT74-05-006","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 03 DEEP 01 BASE (STEERING WHEEL OPERATED).\n2103mm high x 2760mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","North West"]
[522,"RT74-05-006","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 03 DEEP 01 BASE (STEERING WHEEL OPERATED).\n2103mm high x 2760mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","Western Cape"]
[523,"RT74-05-007","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 04 DEEP 03 BASES (STEERING WHEEL OPERATED). \n2103mm high x 3680mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Eastern Cape"]
[524,"RT74-05-007","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 04 DEEP 03 BASES (STEERING WHEEL OPERATED). \n2103mm high x 3680mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Free State"]
[525,"RT74-05-007","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 04 DEEP 03 BASES (STEERING WHEEL OPERATED). \n2103mm high x 3680mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Gauteng"]
[526,"RT74-05-007","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 04 DEEP 03 BASES (STEERING WHEEL OPERATED). \n2103mm high x 3680mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Kwazulu-Natal"]
[527,"RT74-05-007","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 04 DEEP 03 BASES (STEERING WHEEL OPERATED). \n2103mm high x 3680mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Limpopo"]
[528,"RT74-05-007","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 04 DEEP 03 BASES (STEERING WHEEL OPERATED). \n2103mm high x 3680mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Mpumalanga"]
[529,"RT74-05-007","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 04 DEEP 03 BASES (STEERING WHEEL OPERATED). \n2103mm high x 3680mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Northern Cape"]
[530,"RT74-05-007","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 04 DEEP 03 BASES (STEERING WHEEL OPERATED). \n2103mm high x 3680mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","North West"]
[531,"RT74-05-007","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 04 DEEP 03 BASES (STEERING WHEEL OPERATED). \n2103mm high x 3680mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Western Cape"]
[532,"RT74-05-008","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 04 DEEP 01 BASE (STEERING WHEEL OPERATED). \n 2103mm high x 3680mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","Eastern Cape"]
[533,"RT74-05-008","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 04 DEEP 01 BASE (STEERING WHEEL OPERATED). \n 2103mm high x 3680mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","Free State"]
[534,"RT74-05-008","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 04 DEEP 01 BASE (STEERING WHEEL OPERATED). \n 2103mm high x 3680mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","Gauteng"]
[535,"RT74-05-008","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 04 DEEP 01 BASE (STEERING WHEEL OPERATED). \n 2103mm high x 3680mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","Kwazulu-Natal"]
[536,"RT74-05-008","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 04 DEEP 01 BASE (STEERING WHEEL OPERATED). \n 2103mm high x 3680mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","Limpopo"]
[537,"RT74-05-008","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 04 DEEP 01 BASE (STEERING WHEEL OPERATED). \n 2103mm high x 3680mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","Mpumalanga"]
[538,"RT74-05-008","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 04 DEEP 01 BASE (STEERING WHEEL OPERATED). \n 2103mm high x 3680mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","Northern Cape"]
[539,"RT74-05-008","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 04 DEEP 01 BASE (STEERING WHEEL OPERATED). \n 2103mm high x 3680mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","North West"]
[540,"RT74-05-008","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 04 DEEP 01 BASE (STEERING WHEEL OPERATED). \n 2103mm high x 3680mm wide x 381mm deep. 6 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","Western Cape"]
[541,"RT74-05-009","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 01 DEEP 03 BASES (HANDLE OPERATED). \n2484mm high x 920mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Eastern Cape"]
[542,"RT74-05-009","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 01 DEEP 03 BASES (HANDLE OPERATED). \n2484mm high x 920mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Free State"]
[543,"RT74-05-009","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 01 DEEP 03 BASES (HANDLE OPERATED). \n2484mm high x 920mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Gauteng"]
[544,"RT74-05-009","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 01 DEEP 03 BASES (HANDLE OPERATED). \n2484mm high x 920mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Kwazulu-Natal"]
[545,"RT74-05-009","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 01 DEEP 03 BASES (HANDLE OPERATED). \n2484mm high x 920mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Limpopo"]
[546,"RT74-05-009","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 01 DEEP 03 BASES (HANDLE OPERATED). \n2484mm high x 920mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Mpumalanga"]
[547,"RT74-05-009","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 01 DEEP 03 BASES (HANDLE OPERATED). \n2484mm high x 920mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Northern Cape"]
[548,"RT74-05-009","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 01 DEEP 03 BASES (HANDLE OPERATED). \n2484mm high x 920mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","North West"]
[549,"RT74-05-009","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 01 DEEP 03 BASES (HANDLE OPERATED). \n2484mm high x 920mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Western Cape"]
[550,"RT74-05-010","Not Applicable","Mobile Shelving","ADDITIONAL MOBILE FILING SYSTEM 01 DEEP 01 BASE (HANDLE OPERATED).\n2484mm high x 920mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","Eastern Cape"]
[551,"RT74-05-010","Not Applicable","Mobile Shelving","ADDITIONAL MOBILE FILING SYSTEM 01 DEEP 01 BASE (HANDLE OPERATED).\n2484mm high x 920mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","Free State"]
[552,"RT74-05-010","Not Applicable","Mobile Shelving","ADDITIONAL MOBILE FILING SYSTEM 01 DEEP 01 BASE (HANDLE OPERATED).\n2484mm high x 920mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","Gauteng"]
[553,"RT74-05-010","Not Applicable","Mobile Shelving","ADDITIONAL MOBILE FILING SYSTEM 01 DEEP 01 BASE (HANDLE OPERATED).\n2484mm high x 920mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","Kwazulu-Natal"]
[554,"RT74-05-010","Not Applicable","Mobile Shelving","ADDITIONAL MOBILE FILING SYSTEM 01 DEEP 01 BASE (HANDLE OPERATED).\n2484mm high x 920mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","Limpopo"]
[555,"RT74-05-010","Not Applicable","Mobile Shelving","ADDITIONAL MOBILE FILING SYSTEM 01 DEEP 01 BASE (HANDLE OPERATED).\n2484mm high x 920mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","Mpumalanga"]
[556,"RT74-05-010","Not Applicable","Mobile Shelving","ADDITIONAL MOBILE FILING SYSTEM 01 DEEP 01 BASE (HANDLE OPERATED).\n2484mm high x 920mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","Northern Cape"]
[557,"RT74-05-010","Not Applicable","Mobile Shelving","ADDITIONAL MOBILE FILING SYSTEM 01 DEEP 01 BASE (HANDLE OPERATED).\n2484mm high x 920mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","North West"]
[558,"RT74-05-010","Not Applicable","Mobile Shelving","ADDITIONAL MOBILE FILING SYSTEM 01 DEEP 01 BASE (HANDLE OPERATED).\n2484mm high x 920mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","Western Cape"]
[559,"RT74-05-011","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 02 DEEP 03 BASES (HANDLE OPERATED). \n2484mm high x 1840mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Eastern Cape"]
[560,"RT74-05-011","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 02 DEEP 03 BASES (HANDLE OPERATED). \n2484mm high x 1840mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Free State"]
[561,"RT74-05-011","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 02 DEEP 03 BASES (HANDLE OPERATED). \n2484mm high x 1840mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Gauteng"]
[562,"RT74-05-011","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 02 DEEP 03 BASES (HANDLE OPERATED). \n2484mm high x 1840mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Kwazulu-Natal"]
[563,"RT74-05-011","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 02 DEEP 03 BASES (HANDLE OPERATED). \n2484mm high x 1840mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Limpopo"]
[564,"RT74-05-011","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 02 DEEP 03 BASES (HANDLE OPERATED). \n2484mm high x 1840mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Mpumalanga"]
[565,"RT74-05-011","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 02 DEEP 03 BASES (HANDLE OPERATED). \n2484mm high x 1840mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Northern Cape"]
[566,"RT74-05-011","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 02 DEEP 03 BASES (HANDLE OPERATED). \n2484mm high x 1840mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","North West"]
[567,"RT74-05-011","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 02 DEEP 03 BASES (HANDLE OPERATED). \n2484mm high x 1840mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Western Cape"]
[568,"RT74-05-012","Not Applicable","Mobile Shelving","ADDITIONAL MOBILE FILING SYSTEM 02 DEEP 01 BASE (HANDLE OPERATED). \n2484mm high x 1840mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base.\n","Eastern Cape"]
[569,"RT74-05-012","Not Applicable","Mobile Shelving","ADDITIONAL MOBILE FILING SYSTEM 02 DEEP 01 BASE (HANDLE OPERATED). \n2484mm high x 1840mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base.\n","Free State"]
[570,"RT74-05-012","Not Applicable","Mobile Shelving","ADDITIONAL MOBILE FILING SYSTEM 02 DEEP 01 BASE (HANDLE OPERATED). \n2484mm high x 1840mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base.\n","Gauteng"]
[571,"RT74-05-012","Not Applicable","Mobile Shelving","ADDITIONAL MOBILE FILING SYSTEM 02 DEEP 01 BASE (HANDLE OPERATED). \n2484mm high x 1840mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base.\n","Kwazulu-Natal"]
[572,"RT74-05-012","Not Applicable","Mobile Shelving","ADDITIONAL MOBILE FILING SYSTEM 02 DEEP 01 BASE (HANDLE OPERATED). \n2484mm high x 1840mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base.\n","Limpopo"]
[573,"RT74-05-012","Not Applicable","Mobile Shelving","ADDITIONAL MOBILE FILING SYSTEM 02 DEEP 01 BASE (HANDLE OPERATED). \n2484mm high x 1840mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base.\n","Mpumalanga"]
[574,"RT74-05-012","Not Applicable","Mobile Shelving","ADDITIONAL MOBILE FILING SYSTEM 02 DEEP 01 BASE (HANDLE OPERATED). \n2484mm high x 1840mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base.\n","Northern Cape"]
[575,"RT74-05-012","Not Applicable","Mobile Shelving","ADDITIONAL MOBILE FILING SYSTEM 02 DEEP 01 BASE (HANDLE OPERATED). \n2484mm high x 1840mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base.\n","North West"]
[576,"RT74-05-012","Not Applicable","Mobile Shelving","ADDITIONAL MOBILE FILING SYSTEM 02 DEEP 01 BASE (HANDLE OPERATED). \n2484mm high x 1840mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base.\n","Western Cape"]
[577,"RT74-05-013","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 03 DEEP 03 BASES (STEERING WHEEL OPERATED).\n2484mm high x 2760mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Eastern Cape"]
[578,"RT74-05-013","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 03 DEEP 03 BASES (STEERING WHEEL OPERATED).\n2484mm high x 2760mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Free State"]
[579,"RT74-05-013","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 03 DEEP 03 BASES (STEERING WHEEL OPERATED).\n2484mm high x 2760mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Gauteng"]
[580,"RT74-05-013","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 03 DEEP 03 BASES (STEERING WHEEL OPERATED).\n2484mm high x 2760mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Kwazulu-Natal"]
[581,"RT74-05-013","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 03 DEEP 03 BASES (STEERING WHEEL OPERATED).\n2484mm high x 2760mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Limpopo"]
[582,"RT74-05-013","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 03 DEEP 03 BASES (STEERING WHEEL OPERATED).\n2484mm high x 2760mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Mpumalanga"]
[583,"RT74-05-013","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 03 DEEP 03 BASES (STEERING WHEEL OPERATED).\n2484mm high x 2760mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Northern Cape"]
[584,"RT74-05-013","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 03 DEEP 03 BASES (STEERING WHEEL OPERATED).\n2484mm high x 2760mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","North West"]
[585,"RT74-05-013","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 03 DEEP 03 BASES (STEERING WHEEL OPERATED).\n2484mm high x 2760mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Western Cape"]
[586,"RT74-05-014","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 03 DEEP 01 BASE (STEERING WHEEL OPERATED). \n2484mm high x 2760mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","Eastern Cape"]
[587,"RT74-05-014","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 03 DEEP 01 BASE (STEERING WHEEL OPERATED). \n2484mm high x 2760mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","Free State"]
[588,"RT74-05-014","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 03 DEEP 01 BASE (STEERING WHEEL OPERATED). \n2484mm high x 2760mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","Gauteng"]
[589,"RT74-05-014","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 03 DEEP 01 BASE (STEERING WHEEL OPERATED). \n2484mm high x 2760mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","Kwazulu-Natal"]
[590,"RT74-05-014","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 03 DEEP 01 BASE (STEERING WHEEL OPERATED). \n2484mm high x 2760mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","Limpopo"]
[591,"RT74-05-014","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 03 DEEP 01 BASE (STEERING WHEEL OPERATED). \n2484mm high x 2760mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","Mpumalanga"]
[592,"RT74-05-014","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 03 DEEP 01 BASE (STEERING WHEEL OPERATED). \n2484mm high x 2760mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","Northern Cape"]
[593,"RT74-05-014","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 03 DEEP 01 BASE (STEERING WHEEL OPERATED). \n2484mm high x 2760mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","North West"]
[594,"RT74-05-014","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 03 DEEP 01 BASE (STEERING WHEEL OPERATED). \n2484mm high x 2760mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","Western Cape"]
[595,"RT74-05-015","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 04 DEEP 03 BASES (STEERING WHEEL OPERATED). \n2484mm high x 3680mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Eastern Cape"]
[596,"RT74-05-015","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 04 DEEP 03 BASES (STEERING WHEEL OPERATED). \n2484mm high x 3680mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Free State"]
[597,"RT74-05-015","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 04 DEEP 03 BASES (STEERING WHEEL OPERATED). \n2484mm high x 3680mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Gauteng"]
[598,"RT74-05-015","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 04 DEEP 03 BASES (STEERING WHEEL OPERATED). \n2484mm high x 3680mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Kwazulu-Natal"]
[599,"RT74-05-015","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 04 DEEP 03 BASES (STEERING WHEEL OPERATED). \n2484mm high x 3680mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Limpopo"]
[600,"RT74-05-015","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 04 DEEP 03 BASES (STEERING WHEEL OPERATED). \n2484mm high x 3680mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Mpumalanga"]
[601,"RT74-05-015","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 04 DEEP 03 BASES (STEERING WHEEL OPERATED). \n2484mm high x 3680mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Northern Cape"]
[602,"RT74-05-015","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 04 DEEP 03 BASES (STEERING WHEEL OPERATED). \n2484mm high x 3680mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","North West"]
[603,"RT74-05-015","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 04 DEEP 03 BASES (STEERING WHEEL OPERATED). \n2484mm high x 3680mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single static bases , 1 x single movable base , 1 x single lockable base and 1 x 800mm passage. 1mm thick colled rolled steel\n","Western Cape"]
[604,"RT74-05-016","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 04 DEEP 01 BASE (STEERING WHEEL OPERATED). \n2484mm high x 3680mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","Eastern Cape"]
[605,"RT74-05-016","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 04 DEEP 01 BASE (STEERING WHEEL OPERATED). \n2484mm high x 3680mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","Free State"]
[606,"RT74-05-016","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 04 DEEP 01 BASE (STEERING WHEEL OPERATED). \n2484mm high x 3680mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","Gauteng"]
[607,"RT74-05-016","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 04 DEEP 01 BASE (STEERING WHEEL OPERATED). \n2484mm high x 3680mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","Kwazulu-Natal"]
[608,"RT74-05-016","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 04 DEEP 01 BASE (STEERING WHEEL OPERATED). \n2484mm high x 3680mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","Limpopo"]
[609,"RT74-05-016","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 04 DEEP 01 BASE (STEERING WHEEL OPERATED). \n2484mm high x 3680mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","Mpumalanga"]
[610,"RT74-05-016","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 04 DEEP 01 BASE (STEERING WHEEL OPERATED). \n2484mm high x 3680mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","Northern Cape"]
[611,"RT74-05-016","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 04 DEEP 01 BASE (STEERING WHEEL OPERATED). \n2484mm high x 3680mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","North West"]
[612,"RT74-05-016","Not Applicable","Mobile Shelving","MOBILE FILING SYSTEM 04 DEEP 01 BASE (STEERING WHEEL OPERATED). \n2484mm high x 3680mm wide x 381mm deep. 7 x shelves to the height\nUnit has back panels and side panels\nUnit consists of 1 x single movable base\n","Western Cape"]
[613,"RT74-06-001","Not Applicable","Filing Cupboards","2 Door , 4 Shelf Steel Filing Cupboard, two tone, name tag holder, lockable\nDimensions: 450 mm(d) X 900 mm(w)X 1800(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","Eastern Cape"]
[614,"RT74-06-001","Not Applicable","Filing Cupboards","2 Door , 4 Shelf Steel Filing Cupboard, two tone, name tag holder, lockable\nDimensions: 450 mm(d) X 900 mm(w)X 1800(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","Free State"]
[615,"RT74-06-001","Not Applicable","Filing Cupboards","2 Door , 4 Shelf Steel Filing Cupboard, two tone, name tag holder, lockable\nDimensions: 450 mm(d) X 900 mm(w)X 1800(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","Gauteng"]
[616,"RT74-06-001","Not Applicable","Filing Cupboards","2 Door , 4 Shelf Steel Filing Cupboard, two tone, name tag holder, lockable\nDimensions: 450 mm(d) X 900 mm(w)X 1800(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","Kwazulu-Natal"]
[617,"RT74-06-001","Not Applicable","Filing Cupboards","2 Door , 4 Shelf Steel Filing Cupboard, two tone, name tag holder, lockable\nDimensions: 450 mm(d) X 900 mm(w)X 1800(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","Limpopo"]
[618,"RT74-06-001","Not Applicable","Filing Cupboards","2 Door , 4 Shelf Steel Filing Cupboard, two tone, name tag holder, lockable\nDimensions: 450 mm(d) X 900 mm(w)X 1800(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","Mpumalanga"]
[619,"RT74-06-001","Not Applicable","Filing Cupboards","2 Door , 4 Shelf Steel Filing Cupboard, two tone, name tag holder, lockable\nDimensions: 450 mm(d) X 900 mm(w)X 1800(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","Northern Cape"]
[620,"RT74-06-001","Not Applicable","Filing Cupboards","2 Door , 4 Shelf Steel Filing Cupboard, two tone, name tag holder, lockable\nDimensions: 450 mm(d) X 900 mm(w)X 1800(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","North West"]
[621,"RT74-06-001","Not Applicable","Filing Cupboards","2 Door , 4 Shelf Steel Filing Cupboard, two tone, name tag holder, lockable\nDimensions: 450 mm(d) X 900 mm(w)X 1800(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","Western Cape"]
[622,"RT74-06-002","Not Applicable","Filing Cupboards","2 Door, 3 Shelf Steel Filing Cupboard, two tone, name tag holder, lockable\nDimensions: 450 mm(d) X 900mm(w)X 1500(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","Eastern Cape"]
[623,"RT74-06-002","Not Applicable","Filing Cupboards","2 Door, 3 Shelf Steel Filing Cupboard, two tone, name tag holder, lockable\nDimensions: 450 mm(d) X 900mm(w)X 1500(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","Free State"]
[624,"RT74-06-002","Not Applicable","Filing Cupboards","2 Door, 3 Shelf Steel Filing Cupboard, two tone, name tag holder, lockable\nDimensions: 450 mm(d) X 900mm(w)X 1500(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","Gauteng"]
[625,"RT74-06-002","Not Applicable","Filing Cupboards","2 Door, 3 Shelf Steel Filing Cupboard, two tone, name tag holder, lockable\nDimensions: 450 mm(d) X 900mm(w)X 1500(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","Kwazulu-Natal"]
[626,"RT74-06-002","Not Applicable","Filing Cupboards","2 Door, 3 Shelf Steel Filing Cupboard, two tone, name tag holder, lockable\nDimensions: 450 mm(d) X 900mm(w)X 1500(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","Limpopo"]
[627,"RT74-06-002","Not Applicable","Filing Cupboards","2 Door, 3 Shelf Steel Filing Cupboard, two tone, name tag holder, lockable\nDimensions: 450 mm(d) X 900mm(w)X 1500(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","Mpumalanga"]
[628,"RT74-06-002","Not Applicable","Filing Cupboards","2 Door, 3 Shelf Steel Filing Cupboard, two tone, name tag holder, lockable\nDimensions: 450 mm(d) X 900mm(w)X 1500(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","Northern Cape"]
[629,"RT74-06-002","Not Applicable","Filing Cupboards","2 Door, 3 Shelf Steel Filing Cupboard, two tone, name tag holder, lockable\nDimensions: 450 mm(d) X 900mm(w)X 1500(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","North West"]
[630,"RT74-06-002","Not Applicable","Filing Cupboards","2 Door, 3 Shelf Steel Filing Cupboard, two tone, name tag holder, lockable\nDimensions: 450 mm(d) X 900mm(w)X 1500(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","Western Cape"]
[631,"RT74-06-003","Not Applicable","Filing Cupboards","2 Door, 2 Shelf Steel Filing Cupboard, two tone, name tag holder, lockable\nDimensions: 450 mm(d) X 900mm(w)X 900(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","Eastern Cape"]
[632,"RT74-06-003","Not Applicable","Filing Cupboards","2 Door, 2 Shelf Steel Filing Cupboard, two tone, name tag holder, lockable\nDimensions: 450 mm(d) X 900mm(w)X 900(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","Free State"]
[633,"RT74-06-003","Not Applicable","Filing Cupboards","2 Door, 2 Shelf Steel Filing Cupboard, two tone, name tag holder, lockable\nDimensions: 450 mm(d) X 900mm(w)X 900(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","Gauteng"]
[634,"RT74-06-003","Not Applicable","Filing Cupboards","2 Door, 2 Shelf Steel Filing Cupboard, two tone, name tag holder, lockable\nDimensions: 450 mm(d) X 900mm(w)X 900(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","Kwazulu-Natal"]
[635,"RT74-06-003","Not Applicable","Filing Cupboards","2 Door, 2 Shelf Steel Filing Cupboard, two tone, name tag holder, lockable\nDimensions: 450 mm(d) X 900mm(w)X 900(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","Limpopo"]
[636,"RT74-06-003","Not Applicable","Filing Cupboards","2 Door, 2 Shelf Steel Filing Cupboard, two tone, name tag holder, lockable\nDimensions: 450 mm(d) X 900mm(w)X 900(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","Mpumalanga"]
[637,"RT74-06-003","Not Applicable","Filing Cupboards","2 Door, 2 Shelf Steel Filing Cupboard, two tone, name tag holder, lockable\nDimensions: 450 mm(d) X 900mm(w)X 900(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","Northern Cape"]
[638,"RT74-06-003","Not Applicable","Filing Cupboards","2 Door, 2 Shelf Steel Filing Cupboard, two tone, name tag holder, lockable\nDimensions: 450 mm(d) X 900mm(w)X 900(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","North West"]
[639,"RT74-06-003","Not Applicable","Filing Cupboards","2 Door, 2 Shelf Steel Filing Cupboard, two tone, name tag holder, lockable\nDimensions: 450 mm(d) X 900mm(w)X 900(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","Western Cape"]
[640,"RT74-07-001","Not Applicable","Filing Cabinets","4 Drawer Steel Filing Cabinet, two tone, name tag holder, lockable\nDimensions: 630 mm(d) X 470mm(w)X 1320(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","Eastern Cape"]
[641,"RT74-07-001","Not Applicable","Filing Cabinets","4 Drawer Steel Filing Cabinet, two tone, name tag holder, lockable\nDimensions: 630 mm(d) X 470mm(w)X 1320(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","Free State"]
[642,"RT74-07-001","Not Applicable","Filing Cabinets","4 Drawer Steel Filing Cabinet, two tone, name tag holder, lockable\nDimensions: 630 mm(d) X 470mm(w)X 1320(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","Gauteng"]
[643,"RT74-07-001","Not Applicable","Filing Cabinets","4 Drawer Steel Filing Cabinet, two tone, name tag holder, lockable\nDimensions: 630 mm(d) X 470mm(w)X 1320(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","Kwazulu-Natal"]
[644,"RT74-07-001","Not Applicable","Filing Cabinets","4 Drawer Steel Filing Cabinet, two tone, name tag holder, lockable\nDimensions: 630 mm(d) X 470mm(w)X 1320(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","Limpopo"]
[645,"RT74-07-001","Not Applicable","Filing Cabinets","4 Drawer Steel Filing Cabinet, two tone, name tag holder, lockable\nDimensions: 630 mm(d) X 470mm(w)X 1320(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","Mpumalanga"]
[646,"RT74-07-001","Not Applicable","Filing Cabinets","4 Drawer Steel Filing Cabinet, two tone, name tag holder, lockable\nDimensions: 630 mm(d) X 470mm(w)X 1320(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","Northern Cape"]
[647,"RT74-07-001","Not Applicable","Filing Cabinets","4 Drawer Steel Filing Cabinet, two tone, name tag holder, lockable\nDimensions: 630 mm(d) X 470mm(w)X 1320(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","North West"]
[648,"RT74-07-001","Not Applicable","Filing Cabinets","4 Drawer Steel Filing Cabinet, two tone, name tag holder, lockable\nDimensions: 630 mm(d) X 470mm(w)X 1320(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","Western Cape"]
[649,"RT74-07-002","Not Applicable","Filing Cabinets","3 Drawer Steel Filing Cabinet, two tone, name tag holder, lockable\nDimensions: 630 mm(d) X 470mm(w)X 1020(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","Eastern Cape"]
[650,"RT74-07-002","Not Applicable","Filing Cabinets","3 Drawer Steel Filing Cabinet, two tone, name tag holder, lockable\nDimensions: 630 mm(d) X 470mm(w)X 1020(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","Free State"]
[651,"RT74-07-002","Not Applicable","Filing Cabinets","3 Drawer Steel Filing Cabinet, two tone, name tag holder, lockable\nDimensions: 630 mm(d) X 470mm(w)X 1020(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","Gauteng"]
[652,"RT74-07-002","Not Applicable","Filing Cabinets","3 Drawer Steel Filing Cabinet, two tone, name tag holder, lockable\nDimensions: 630 mm(d) X 470mm(w)X 1020(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","Kwazulu-Natal"]
[653,"RT74-07-002","Not Applicable","Filing Cabinets","3 Drawer Steel Filing Cabinet, two tone, name tag holder, lockable\nDimensions: 630 mm(d) X 470mm(w)X 1020(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","Limpopo"]
[654,"RT74-07-002","Not Applicable","Filing Cabinets","3 Drawer Steel Filing Cabinet, two tone, name tag holder, lockable\nDimensions: 630 mm(d) X 470mm(w)X 1020(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","Mpumalanga"]
[655,"RT74-07-002","Not Applicable","Filing Cabinets","3 Drawer Steel Filing Cabinet, two tone, name tag holder, lockable\nDimensions: 630 mm(d) X 470mm(w)X 1020(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","Northern Cape"]
[656,"RT74-07-002","Not Applicable","Filing Cabinets","3 Drawer Steel Filing Cabinet, two tone, name tag holder, lockable\nDimensions: 630 mm(d) X 470mm(w)X 1020(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","North West"]
[657,"RT74-07-002","Not Applicable","Filing Cabinets","3 Drawer Steel Filing Cabinet, two tone, name tag holder, lockable\nDimensions: 630 mm(d) X 470mm(w)X 1020(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","Western Cape"]
[658,"RT74-07-003","Not Applicable","Filing Cabinets","2 Drawer Steel Filing Cabinet, two tone, name tag holder, lockable\nDimensions: 630 mm(d) X 470mm(w)X 720(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","Eastern Cape"]
[659,"RT74-07-003","Not Applicable","Filing Cabinets","2 Drawer Steel Filing Cabinet, two tone, name tag holder, lockable\nDimensions: 630 mm(d) X 470mm(w)X 720(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","Free State"]
[660,"RT74-07-003","Not Applicable","Filing Cabinets","2 Drawer Steel Filing Cabinet, two tone, name tag holder, lockable\nDimensions: 630 mm(d) X 470mm(w)X 720(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","Gauteng"]
[661,"RT74-07-003","Not Applicable","Filing Cabinets","2 Drawer Steel Filing Cabinet, two tone, name tag holder, lockable\nDimensions: 630 mm(d) X 470mm(w)X 720(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","Kwazulu-Natal"]
[662,"RT74-07-003","Not Applicable","Filing Cabinets","2 Drawer Steel Filing Cabinet, two tone, name tag holder, lockable\nDimensions: 630 mm(d) X 470mm(w)X 720(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","Limpopo"]
[663,"RT74-07-003","Not Applicable","Filing Cabinets","2 Drawer Steel Filing Cabinet, two tone, name tag holder, lockable\nDimensions: 630 mm(d) X 470mm(w)X 720(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","Mpumalanga"]
[664,"RT74-07-003","Not Applicable","Filing Cabinets","2 Drawer Steel Filing Cabinet, two tone, name tag holder, lockable\nDimensions: 630 mm(d) X 470mm(w)X 720(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","Northern Cape"]
[665,"RT74-07-003","Not Applicable","Filing Cabinets","2 Drawer Steel Filing Cabinet, two tone, name tag holder, lockable\nDimensions: 630 mm(d) X 470mm(w)X 720(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","North West"]
[666,"RT74-07-003","Not Applicable","Filing Cabinets","2 Drawer Steel Filing Cabinet, two tone, name tag holder, lockable\nDimensions: 630 mm(d) X 470mm(w)X 720(h) \nMaterial  - Mild Steel\nThickness: 1,2 mm\n","Western Cape"]
[667,"RT74-08-001","Not Applicable","Parcel Trolley","Overall Size (LxWxH): 1100x650x940mm                                                                                                                              ideal for stock picking and transferring boxed products\nElectro galvanised finish\nHeavy duty rubber castors – 2 x fixed, 2 x swivel\nLoad Capacity: 300kg\nCastors: 160mm\nOverall Size (LxWxH): 1100x650x940mm\nUnit Weight: 36kg\n","Eastern Cape"]
[668,"RT74-08-001","Not Applicable","Parcel Trolley","Overall Size (LxWxH): 1100x650x940mm                                                                                                                              ideal for stock picking and transferring boxed products\nElectro galvanised finish\nHeavy duty rubber castors – 2 x fixed, 2 x swivel\nLoad Capacity: 300kg\nCastors: 160mm\nOverall Size (LxWxH): 1100x650x940mm\nUnit Weight: 36kg\n","Free State"]
[669,"RT74-08-001","Not Applicable","Parcel Trolley","Overall Size (LxWxH): 1100x650x940mm                                                                                                                              ideal for stock picking and transferring boxed products\nElectro galvanised finish\nHeavy duty rubber castors – 2 x fixed, 2 x swivel\nLoad Capacity: 300kg\nCastors: 160mm\nOverall Size (LxWxH): 1100x650x940mm\nUnit Weight: 36kg\n","Gauteng"]
[670,"RT74-08-001","Not Applicable","Parcel Trolley","Overall Size (LxWxH): 1100x650x940mm                                                                                                                              ideal for stock picking and transferring boxed products\nElectro galvanised finish\nHeavy duty rubber castors – 2 x fixed, 2 x swivel\nLoad Capacity: 300kg\nCastors: 160mm\nOverall Size (LxWxH): 1100x650x940mm\nUnit Weight: 36kg\n","Kwazulu-Natal"]
[671,"RT74-08-001","Not Applicable","Parcel Trolley","Overall Size (LxWxH): 1100x650x940mm                                                                                                                              ideal for stock picking and transferring boxed products\nElectro galvanised finish\nHeavy duty rubber castors – 2 x fixed, 2 x swivel\nLoad Capacity: 300kg\nCastors: 160mm\nOverall Size (LxWxH): 1100x650x940mm\nUnit Weight: 36kg\n","Limpopo"]
[672,"RT74-08-001","Not Applicable","Parcel Trolley","Overall Size (LxWxH): 1100x650x940mm                                                                                                                              ideal for stock picking and transferring boxed products\nElectro galvanised finish\nHeavy duty rubber castors – 2 x fixed, 2 x swivel\nLoad Capacity: 300kg\nCastors: 160mm\nOverall Size (LxWxH): 1100x650x940mm\nUnit Weight: 36kg\n","Mpumalanga"]
[673,"RT74-08-001","Not Applicable","Parcel Trolley","Overall Size (LxWxH): 1100x650x940mm                                                                                                                              ideal for stock picking and transferring boxed products\nElectro galvanised finish\nHeavy duty rubber castors – 2 x fixed, 2 x swivel\nLoad Capacity: 300kg\nCastors: 160mm\nOverall Size (LxWxH): 1100x650x940mm\nUnit Weight: 36kg\n","Northern Cape"]
[674,"RT74-08-001","Not Applicable","Parcel Trolley","Overall Size (LxWxH): 1100x650x940mm                                                                                                                              ideal for stock picking and transferring boxed products\nElectro galvanised finish\nHeavy duty rubber castors – 2 x fixed, 2 x swivel\nLoad Capacity: 300kg\nCastors: 160mm\nOverall Size (LxWxH): 1100x650x940mm\nUnit Weight: 36kg\n","North West"]
[675,"RT74-08-001","Not Applicable","Parcel Trolley","Overall Size (LxWxH): 1100x650x940mm                                                                                                                              ideal for stock picking and transferring boxed products\nElectro galvanised finish\nHeavy duty rubber castors – 2 x fixed, 2 x swivel\nLoad Capacity: 300kg\nCastors: 160mm\nOverall Size (LxWxH): 1100x650x940mm\nUnit Weight: 36kg\n","Western Cape"]