{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["RFP162.2023"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"RFP162.2023","index":0,"n_rows":18,"n_cols":6,"rows_kept":18,"merged":[[0,0,0,5],[1,1,1,5],[13,0,13,4],[17,0,17,4]]}
["RFP162/2023: \nTHE SUPPLY, CUT, BEND, GALVANIZING AND DELIVERY OF STEEL BARS(REINFORCEMENT) FOR CONCRETE FOR A PERIOD OF UP TO 15 MONTHS TO DWS CONSTRUCTION NORTH TZANEEN DAM RAISING PROJECT IN THE LIMPOPO PROVINCE."]
[]
["Item","Description","Unit","Quantity","Rate","Total"]
[1,"Mild steel"]
["1.1","Supply, cut, bend and delivery of 8 mm, 10 mm, 12 mm, 16 mm and 20 mm of Mild steel bars, of strength 250 Mpa  ","ton",70,null,{"$f":"D5*E5","v":{"v":0,"d":"R0.00"}}]
[2,"High tensile steel"]
["2.1","Supply, cut, bend and delivery of 8 mm, 10 mm, 12 mm, 16 mm 20 mm, 25 mm and 32 mm of High yield deformed steel bars, of strength 450 MPa  ","ton",1500,null,{"$f":"D7*E7","v":{"v":0,"d":"R0.00"}}]
[3,"Galvanized Steel"]
["3.1","Supply, cut, bend, hot – dip galvanizing and delivery of 20 mm, 25 mm and 32 mm of High yield deformed steel bars, of strength 450 Mpa","ton",120,null,{"v":0,"d":"R0.00"}]
[4,"Binding wires, Cover/spacer blocks"]
["4.1","Binding wire - 1.6mm/50 kg","kg",{"v":1800,"d":"1,800"},null,{"v":0,"d":"R0.00"}]
["4.2","Plastic Spacer Blocks - 50 mm","No.",10000,null,{"$f":"D12*E12","v":{"v":0,"d":"R0.00"}}]
["4.3","Grit hand cleaner for reinforcement /1 kg container","No. ",200,null,{"v":0,"d":"R0.00"}]
["TOTAL",{"$nulls":4},{"$f":"SUM(F5:F13)","v":{"v":0,"d":"R0.00"}}]
["Contegency",null,null,{"v":0.1,"d":"10%"},null,{"$f":"F14*D15","v":{"v":0,"d":"R0.00"}}]
["SUB TOTAL",{"$nulls":4},{"$f":"SUM(F14:F15)","v":{"v":0,"d":"R0.00"}}]
["VAT @ 15%",null,null,{"v":0.15,"d":"15%"},null,{"$f":"F16*D17","v":{"v":0,"d":"R0.00"}}]
["GRAND TOTAL",{"$nulls":4},{"$f":"SUM(F16:F17)","v":{"v":0,"d":"R0.00"}}]