{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["SAP - 167508","Deviation Schedule","Test Schedule"],"not_rendered":{"defined_names":7},"read":"whole","date_system":"1900"}

{"sheet":"SAP - 167508","index":0,"n_rows":66,"n_cols":7,"rows_kept":66,"merged":[[0,0,0,6],[1,1,1,6],[2,1,2,6],[3,1,3,6],[4,1,4,6],[7,2,7,3],[8,2,8,3],[9,3,9,4],[19,3,19,4],[25,3,25,4],[31,3,31,4],[34,3,34,4],[38,3,38,4],[41,2,41,4],[42,2,42,4],[43,3,43,4],[46,3,46,4],[57,1,57,3],[59,1,59,6],[60,1,60,6],[62,0,62,1],[63,5,63,6],[65,2,65,3],[65,5,65,6]]}
["ESKOM TENDER E2719DXLIMOU"]
[null,"Technical Schedules A and B for"]
[null,"CLEVIS-BALL 16mm 16L 80CL 120kN D6059"]
[null,"Schedule A:  Purchasers specific requirements"]
[null,"Schedule B:  Guarantees and technical particulars of equipment offered"]
[]
[null,1,null,2,null,3,4]
[null,"Item ","Description",null,null,"Schedule A","Schedule B"]
[null,1,"Product Information"]
[null,1.1,"·","Purchasing details"]
[null,"1.1.1",null,"Eskom SAP No",null,{"v":167508,"d":"0167508"},"xxxxxxxxxx"]
[null,"1.1.2",null,"Manufacturer's Name",null,"xxxxxxxxxx"]
[null,"1.1.3",null,"Manufacturer's Product Code",null,"xxxxxxxxxx"]
[null,"1.1.4",null,"Manufacturer's Drawing number & Revision number",null,"xxxxxxxxxx"]
[null,"1.1.5",null,"Manufacturer's Physical identification mark on product",null,"xxxxxxxxxx"]
[null,"1.1.6",null,"Compliance to all dimensions and requirements of Eskom Buyer's Guide drawing","D-DT 6059","YES"]
[null,"1.1.7",null,"Item sample required, upon request from Eskom. (As per the Technical Criteria Document)",null,"YES","xxxxxxxxxx"]
[null,"1.1.8",null,"Item supplied complete with:\n1 x M16x75 Clevis bolt assembly (D-DT-7043)",null,"YES"]
[]
[null,1.2,"·","Mechanical Properties"]
[null,"1.2.1",null,"Mechanical failing load","kN",120]
[null,"1.2.2",null,"Material Grade Clevis Ball",null,"Drop Forged Steel EN8 (080M40)"]
[null,"1.2.3",null,"Material Grade Bolt",null,"Steel Grade 4.8 "]
[null,"1.2.4",null,"Material Grade Split Pin",null,"Stainless Steel Grade 304"]
[]
[null,1.3,"·","Material Dimensions"]
[null,"1.3.1",null,"Coupling Length","mm",80]
[null,"1.3.2",null,"Clevis Opening","mm",18]
[null,"1.3.3",null,"Ball dimensions to SANS 60120",null,16]
[null,"1.3.4",null,"Clevis dimensions to SANS 60471",null,"16L"]
[null,"1.3.5",null,"Locking devise: \n- Hump back split pin to 240-75883164",null,"YES"]
[{"$nulls":3},"Accessories"]
[null,"1.3.6",null," - 1 x M16x75 Clevis bolt assembly (D-DT-7043) complete with: \n        1 x M16x75 bolt, \n        1 x flat washer, \n        1 x hump back split pin","mm","M16x75"]
[]
[null,1.4,"·","Hot-dip Galvanizing"]
[null,"1.4.1",null,"Average minimum galvanising thickness on product body to SANS 121","µm","YES"]
[null,"1.4.2",null,"Average minimum galvanising thickness on product accessories supplied (bolt, washer & nut) to SANS 121","µm","YES"]
[]
[null,1.5,"·","Packaging"]
[null,"1.5.1",null,"All items packaged as a unit (including accessories) - packaging suitable for outdoor storage",null,"YES"]
[]
[null,2,"Documentation (to be submitted with tender)"]
[null,null,"Note:  All documentation to be provided in electronic format."]
[null,2.1,"·","General"]
[null,"2.1.1",null,"Outline drawings of item","Sets",1]
[null,"2.1.2",null,"Material grade certification","Certification submitted","YES"]
[null,2.2,"·","Test Reports (where applicable)",null,"Required","Report Number"]
[null,"2.2.1",null,"Visual examination (SANS 61284)","Test report submitted","YES"]
[null,"2.2.2",null,"Dimensional and material verification (SANS 61284)","Test report submitted","YES"]
[null,"2.2.3",null,"Hot dip galvanizing (SANS 121)","Test report submitted","YES"]
[null,"2.2.4",null,"Mechanical Test \n- Mechanical Damage and Failure load test (SANS 61284: with SMDL = 67% of SMFL)","Test report submitted","YES"]
[null,"2.2.5",null," - Clamp Bolt Tightening test (SANS 61284)","Test report submitted","YES"]
[null,"2.2.6",null," - Tensile Test (SANS 61284)","Test report submitted","YES"]
[null,"2.2.7",null,"Non-destructive Testing:\n - Hardness Test (SANS 61284)","Test report submitted","YES"]
[null,"2.2.8",null,"Heat Cycle Test (SANS 61284)","Test report submitted","YES"]
[null,"2.2.9",null,"Pull test for hump back split pin (240-75883164)","Test report submitted","YES"]
[]
[]
[{"$nulls":3},"ESKOM TENDER E2719DXLIMOU"]
[null,"NOTE:  DEVIATION SCHEDULE CONTINUE ON NEXT PAGE.\n             IF NO DEVIATIONS ARE MENTIONED ON THE DEVIATION SCHEDULE IT WILL BE ACCEPTED THAT THE SUPPLIER\n              AND MANUFACTURER FULLY COMPLIES WITH THE REQUIREMENTS OF THE ESKOM SPECIFICATON(S)."]
[null,"SUPPLIER SIGNATURES"]
[]
[null,null,"         "]
[{"$nulls":3},"Name (Print)",null,"Company Name"]
[]
[null,null,"Sign",null,null,"Date"]

{"sheet":"Deviation Schedule","index":1,"n_rows":43,"n_cols":5,"rows_kept":43,"merged":[[0,0,0,6],[1,0,1,6],[2,1,2,5],[3,1,3,3],[4,0,4,6],[5,2,5,6],[6,2,6,6],[7,2,7,6],[8,2,8,6],[9,2,9,6],[10,2,10,6],[11,2,11,6],[12,2,12,6],[13,2,13,6],[14,2,14,6],[15,2,15,6],[16,2,16,6],[17,2,17,6],[18,2,18,6],[19,2,19,6],[20,2,20,6],[21,2,21,6],[22,2,22,6],[23,2,23,6],[24,2,24,6],[25,2,25,6],[26,2,26,6],[27,2,27,6],[28,2,28,6],[29,2,29,6],[30,2,30,6],[31,2,31,6],[32,2,32,6],[33,2,33,6],[34,2,34,6],[35,2,35,6],[36,0,36,6],[38,0,38,1],[39,0,39,1],[39,4,39,5],[42,4,42,5]]}
["ESKOM TENDER E2719DXLIMOU"]
["Deviation schedule (DDT 6059)"]
[null,"DESCRIPTION:"]
[null,"SAP:  167508"]
["Any deviations offered to this specification shall be listed below with reasons for deviation.  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective that that specified by Eskom."]
["Item","Clause","Description of Deviation"]
{"$rows_empty":30}
["SUPPLIER SIGNATURES"]
[]
[null,null,"         "]
[null,null,"Name (Print)",null,"Company Name"]
[]
[null,null,"         "]
[null,null,"Sign",null,"Date"]

{"sheet":"Test Schedule","index":2,"n_rows":26,"n_cols":7,"rows_kept":26,"merged":[[0,0,0,6],[1,1,1,6],[2,1,2,3],[3,1,3,2],[6,2,6,3],[18,0,18,6],[20,0,20,1],[21,5,21,6],[25,2,25,3],[25,5,25,6]]}
["ESKOM TENDER E2719DXLIMOU"]
[null,"Test Report Schedule for DDT 6059"]
[null,"DESCRIPTION:",null,null,"SAP:",{"v":167508,"d":"0167508"}]
[]
[]
[null,1,null,2,null,3,4]
[null,"Item ","Description",null,"Test","Specification","Report Number"]
[null,"2.2.1",null,"Visual examination","Type","SANS 61284"]
[null,"2.2.2",null,"Dimensional and material verification","Type","SANS 61284"]
[null,"2.2.3",null,"Hot dip galvanizing","Sample","SANS 121"]
[null,"2.2.4",null,"Mechanical Test \n- Mechanical Damage and Failure load test (SANS 61284: with SMDL = 67% of SMFL)","Sample","SANS 61284"]
[null,"2.2.5",null," - Clamp Bolt Tightening test","Sample","SANS 61284"]
[null,"2.2.6",null," - Tensile Test","Sample","SANS 61284"]
[null,"2.2.7",null,"Non-destructive Testing:\n - Hardness Test","Sample","SANS 61284"]
[null,"2.2.8",null,"Heat Cycle Test","Sample","SANS 61284"]
[null,"2.2.9",null,"Pull test for hump back split pin (240-75883164)","Sample","240-75883164"]
[]
[]
["SUPPLIER SIGNATURES"]
[]
[null,null,"         "]
[{"$nulls":3},"Name (Print)",null,"Company Name"]
[]
[]
[]
[null,null,"Sign",null,null,"Date"]