{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["MGS-02-07-04"],"read":"whole","date_system":"1900"}

{"sheet":"MGS-02-07-04","index":0,"n_rows":1630,"n_cols":157,"rows_kept":1630}
[null,"DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT"]
[]
[null,"SECTION NO. 1","H1"]
[]
[null,"BILL NO. 1","H1"]
[]
[null,"PRELIMINARIES","H1"]
[]
[null,"BUILDING AGREEMENT AND PRELIMINARIES","H2"]
[]
[null,"The  JBCC Principal Building Agreement (May 2018 Edition 6.2) prepared by the Joint Building Contracts Committee shall be the applicable building agreement, amended as hereinafter described"]
[]
[null,"The JBCC Principal Building Agreement contract data form an integral part of this agreement"]
[]
[null,"The Preliminaries revision 1 (February 2016) published by the Association of South African Quantity Surveyors for use with the JBCC Principal Building Agreement Edition 6.2 shall be deemed to be incorporated in these bills of quantities, amended as hereinafter described"]
[]
[null,"The contractor is deemed to have referred to the abovementioned documents for the full intent and meaning of each clause"]
[]
[null,"The clauses in the abovementioned documents are hereinafter referred to by clause number and heading only"]
[]
[null,"Where any item is not relevant to this agreement such item is marked N/A signifying \"not applicable\""]
[]
[null,"PREAMBLES FOR TRADES","H2"]
[]
[null,"The Model Preambles for Trades 2008 published by the Association of South African Quantity Surveyors is designed to support and extend the abbreviated descriptions utilised in these bills of quantities by inter alia referring to SANS construction standards."]
[]
[null,"Note that the text of the Standard System of Measuring Building Work (seventh edition) and that of the Standard Method of Measuring Building Work for Africa 2015 (first edition) is the same"]
[]
[null,"The Model Preambles for Trades 2008 as published by the Association of South African Quantity Surveyors shall be deemed to be incorporated in these bills of quantities and no claims arising from brevity of description of items fully described in the said Model Preambles will be entertained"]
[]
[null,"Supplementary preambles and/or specifications are incorporated in these bills of quantities to satisfy the requirements of this project. Such supplementary preambles and/or specifications shall take precedence over the provisions of the Model Preambles"]
[]
[null,"The contractor's prices for all items throughout these bills of quantities shall take account of and include for all of the obligations, requirements and specifications given in the Model Preambles and in any supplementary preambles and/or specifications"]
[]
[null,"NOTES TO TENDERERS","H2"]
[]
[null,"Minimum Threshold for Local Content  Section No.2 - Builder's Work  BILL",{"$nulls":36},"100%  Metal sheeting  ",null,"ROOF SHEETING",2,1,"Roof sheeting pitch no exceeding 18 degrees","100%  "," "," ","  Gutters, downpipes and lauders  "," ","RAINWATER GOODS","  8",1,"PVC gutters with 20mm overlapping joints sealed with and including bitumen impregnated foam plastic joint sealing strip and riveted at 20mm centres","100% 8",2,"80mm PVC down pipe fixed to brick wall including brackets","100% 8",3,"Extra over eaves gutter for offset","100% 8",4,"Extra over eaves gutter for outlet","100% 8",5,"Extra over eaves gutter for stopped end","100% 8",6,"Extra over for shoe","100%  "," "," ","   Section No.2 - Builder's Work (Wet Services)  BILL","Item","Description","Threshold SANITARY PLUMBING 8","2022-12-14","Class 34 uPVC Pipe","100% 8","15-27","Class 34 uPVC FITTINGS",{"v":1,"d":"100%"},null,null," WATER SUPPLY - COLD WATER RETICULATION  "," ","Replace defective pipe sections and fittings","  8","28-29","PEX Piping","100% 8","31-33","Extra over PEX pipes for fittings","100% 8","34-36","Plastic Pipe Compression Fittings And Valves","100% 8","37-38","Pipe Hangers - Anchor, Threaded Rod & Hanger","100%  Section No.3 - Electrical Installation  BILL","Item","Description","Threshold CABLES AND CONDUCTORS 1","23 & 26","2,5mm conductors (mixed colours - live, neutral and earth). 4,0mm conductors (mixed colours - live, neutral and earth) ","90% 1","23 - 24 & 27 -33","2.5 mm² 2c 600/1000V PVC/SWA/PVC ECC Cu Cable. 4,0 mm² 4c 600/1000V PVC/SWA/PVC ECC Cu Cable. 10 mm² 2c 600/1000V PVC/SWA/PVC ECC Cu Cable. 10 mm² 4c 600/1000V PVC/SWA/PVC ECC Cu Cable. 25 mm² 4c 600/1000V PVC/SWA/PVC ECC Cu Cable. ","90% 1","63, 71 & 75","50 mm² 4c 600/1000V PVC/SWA/PVC ECC Cu Cable","90% 1",67,"95 mm² 4c 600/1000V PVC/SWA/PVC ECC Cu Cable","  "," "," ","  TRUNKING, POWER SKIRTING & CONDUITS 1",34,"25mm PVC Conduit including all necessary accessories.32mm steel Conduit including all necessary accessories.","100% 1","35-36","25mm steel Conduit including all necessary accessories.32mm steel Conduit including all necessary accessories. 32mm steel Conduit including all necessary accessories.32mm steel Conduit including all necessary accessories.","100%  Section No.4 - Fire Protection  BILL","Item","Description","Threshold Supply, deliver and install all Fire appliances and piping with complete with all auxiliary fittings :. 1","2022-07-10","Black Mild Steel Fittings","100% 1","2022-11-12","Black Mild Steel Piping","100% 1","13-19","Class 16 HDPE Piping & Fittings","100%  Section No.5 - HVAC Installation  BILL","Item","Description","Threshold Supply, deliver and install the following Units as per specification: 1",11,"Refrigeration Copper Piping With Thermal Insulation and all associated Fittings.","100% 1",12,"PVC Condensate Drain Piping With Insulation","100% 1",16,"Fabricate , Supply and Install lockable Security Cages around each Outdoor Condensing Unit",{"v":1,"d":"100%"},"17-26","Supply The following Ablution Extraction System with Complete Associated Fittings",{"v":1,"d":"100%"},null,0,{"$nulls":4},"01/12/2022 06:47:59"]
[]
[null,"Tenderers are to inspect the drawings issued with these Bills of Quantities and to satisfy themselves with the nature and the requirements of the Contract works. Failure to do so will be the complete responsibility of the Tenderer and no claims whatsoever will be entertained in this regard."]
[]
[null,"Tenderers are to read the descriptions, which are intended as a means of identifying various facets of the work, in conjunction with the drawings. Tenderers shall allow for all costs in connection with the various items taking full cognisance of both the drawings and the Bills of Quantities. "]
[]
[null,"Tenderers shall notify the Quantity Surveyor in writing of any discrepancies encountered upon which clarification will be given by the Quantity Surveyor in writing to the Tenderer. Failure to do so will be the complete responsibility of the Tenderer and no claims whatsoever will be entertained in this regard"]
[]
[null,"Tenderers are to note that setting out of the works will be the complete responsibility of the Tenderer and they should therefore acquaint themselves with the site boundaries, site co-ordinates, datum levels etc. Failure to do so will be the complete responsibility of the Tenderer and no claims whatsoever will be entertained in this regard.  Tenderers are to note that all items with ZERO quantities are Rate Only items and should be priced as such."]
[]
[null,"Tenderers are to note that there might be specified suppliers to be used for certain trades as per the annexure to this tender document. Tenderers should familiarise themselves with the suppliers on the list and ensure to allow for accordingly. Failure to do so will be the complete responsibility of the Tenderer and no claims whatsoever will be entertained in this regard."]
[]
[null,"Tenderers are to fully acquaint themselves with the construction period and shall allow for any night shift if required. Failure to do so will be the complete responsibility of the Tenderer and no claims whatsoever will be entertained in this regard."]
[]
[null,"STRUCTURE OF THIS PRELIMINARIES BILL","H2"]
[]
[null,"Section A : A recital of the headings of the individual clauses of the aforementioned JBCC Principal Building Agreement"]
[]
[null,"Section B : A recital of the headings of the individual clauses of the aforementioned Preliminaries document"]
[]
[null,"Section C : Any special clauses to meet the particular circumstances of the project"]
[]
[null,"PRICING OF PRELIMINARIES","H2"]
[]
[null,"Should the contractor select Option A in the contract data for the adjustment of preliminaries, the amounts entered against the relevant items in these preliminaries are to be divided into one or more of the three categories provided namely fixed (F), value related (V) and time related (T) "]
[]
[null,"LOCATIONS DESCRIPTIONS: ","H2"]
[]
[null,"QUANTITIES IN THESE BILLS OF QUANTITIES ARE SPLIT INTO THE LOCATIONS:  LOCATION [A] - CONGELLA STATION  LOCATION [B] - UMBILO STATION  LOCATION [C] - ROSSBURGH STATION  LOCATION [D] - MEREBANK STATION"]
[]
[null,"SECTION A: PRINCIPAL BUILDING AGREEMENT","H2"]
[]
[null,"Interpretation (A1-A7)","H3"]
[]
[null,"Clause 1.0 - Definitions and interpretation","CONT"]
[]
[null,"F:............................. V:............................ T:............................","Item",1]
[]
[null,"Clause 2.0 - Law, regulations and notices","CONT",0]
[]
[null,"F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 3.0 - Offer and acceptance  F:............................. V:............................ T:............................ ","Item",0]
[]
[null,"Clause 4.0 - Assignment and cession  F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 5.0 - Contract documents","CONT",0]
[]
[null,"F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 6.0 - Employer's agents","CONT",0]
[]
[null,"1. PRINCIPAL AGENT  LODEMANN HOLDINGS Suite 301 Wheeler House 112-116 Mathews Meyiwa Rd (Stamford Hill) Morningside Durban  ","CONT",0]
[]
[null,"F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 7.0 - Design responsibility  F:............................. V:............................ T:............................","Item",0]
[]
[null,"Insurance and security (A8-A11)","H3",0]
[]
[null,"Clause 8.0 - Works risk  F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 9.0 - Indemnities  F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 10.0 - Insurances  F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 11.0 - Security","CONT",0]
[]
[null,"F:............................. V:............................ T:............................","Item",0]
[]
[null,"Execution (A12 - A17) ","H3",0]
[]
[null,"Clause 12.0 - Duties of the parties","CONT",0]
[]
[null,"F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 13.0 - Setting out  F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 14.0 - Nominated subcontractors","CONT",0]
[]
[null,"F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 15.0 - Selected subcontractors","CONT",0]
[]
[null,"F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 16.0 - Direct contractors  Attendance on direct contractors  In respect of direct contractors the contractor shall:","CONT",0]
[]
[null,"F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 17.0 - Contract instructions  Site instructions  Instructions issued on site are to be recorded in a site instruction book which is to be supplied and maintained on site by the contractor ","CONT",0]
[]
[null,"F:............................. V:............................ T:............................","Item",0]
[]
[null,"Completion (A18 - A24) ","H3",0]
[]
[null,"Clause 18.0 - Interim completion  F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 19.0 - Practical completion   F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 20.0 - Sectional completion ","CONT",0]
[]
[null,"F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 21.0 - Defects liability period and final completion","CONT",0]
[]
[null,"F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 22.0 - Latent defects liability period F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 23.0 - Revision of date for practical completion  Substitution of materials and goods  The removal or substitution of any materials and goods which do not conform to the specification or the contract drawings shall not constitute grounds for the extension of the construction period nor for the adjustment of the contract value [17.1.8, 23.1 & 2]","CONT",0]
[]
[null,"F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 24.0 - Penalty for late or non-completion    F:............................. V:............................ T:............................","Item",0]
[]
[null,"Payment (A25 - A27) ","H3",0]
[]
[null,"Clause 25.0 - Payment","CONT",0]
[]
[null,"F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 26.0 - Adjustment of the contract value and final account","CONT",0]
[]
[null,"F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 27.0 - Recovery of expense and/or loss  F:............................. V:............................ T:............................","Item",0]
[]
[null,"Suspension and termination (A28 - A29) ","H3",0]
[]
[null,"Clause 28.0 - Suspension by the contractor","CONT",0]
[]
[null,"F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 29.0 - Termination","CONT",0]
[]
[null,"F:............................. V:............................ T:............................","Item",0]
[]
[null,"Dispute resolution (A30) ","H3",0]
[]
[null,"Clause 30.0 - Dispute resolution  F:............................. V:............................ T:............................","Item",0]
[]
[null,"The required information of the parties and the amount of the contract sum shall be inserted in the agreement for signature of the agreement by the parties  F:............................. V:............................ T:............................","Item",0]
[]
[null,"F:............................. V:............................ T:............................","Item",0]
[]
[null,"SECTION B:  PRELIMINARIES ","H2",0]
[]
[null,"Interpretation (B1) ","H3",0]
[]
[null,"Clause 1.1 - Definitions  F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 1.2 - Interpretation  F:............................. V:............................ T:............................","Item",0]
[]
[null,"Documents (B2) ","H3",0]
[]
[null,"Clause 2.1 - Checking of documents  F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 2.2 - Provisional bills of quantities","CONT",0]
[]
[null," F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 2.3 - Availability of construction informationBudgetary allowances and provisional sumsThe budgetary allowances and/or provisional sums allocated for subsequent trades included in this agreement will be separately procured, based on multiple procurement of subcontractors during the construction period F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 2.4 - Ordering of materials and goods  F:............................. V:............................ T:............................","Item",0]
[]
[null,"Previous work and adjoining properties (B3) ","H3",0]
[]
[null,"Clause 3.1 - Previous work - dimensional accuracy  F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 3.2 - Previous work - defects  F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 3.3 - Inspection of adjoining properties  F:............................. V:............................ T:............................","Item",0]
[]
[null,"The site (B4) ","H3",0]
[]
[null,"Clause 4.1 - Defined works area  F:............................. V:............................ T:...........................","Item",0]
[]
[null,"Clause 4.2 - Handover of site in stages  F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 4.3 - Enclosure of the works  F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 4.4 - Geotechnical investigation  F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 4.5 - Encroachments  F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 4.6 - Existing premises occupied  F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 4.7 - Services - known  F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 4.8 - Protection of trees and/or relevant natural features  F:............................. V:............................ T:...........................","Item",0]
[]
[null,"Management of contract (B5) ","H3",0]
[]
[null,"Clause 5.1 - Management of the works  F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 5.2 - Progress meetings  F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 5.3 - Technical meetings  F:............................. V:............................ T:............................","Item",0]
[]
[null,"Samples, shop drawings and manufacturer's instructions (B6) ","H3",0]
[]
[null,"Clause 6.1 - Samples of materials  F:............................. V:............................ T:...........................","Item",0]
[]
[null,"Clause 6.2 - Workmanship samples  F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 6.3 - Shop drawings  F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 6.4 - Compliance with manufacturer's instructions  F:............................. V:............................ T:............................","Item",0]
[]
[null,"Deposits and fees (B7) ","H3",0]
[]
[null,"Clause 7.1 - Deposits and fees  F:............................. V:............................ T:............................","Item",0]
[]
[null,"Temporary services (B8) ","H3",0]
[]
[null,"Clause 8.1 - Water  F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 8.2 - Electricity  F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 8.3 - Ablution and welfare facilities  F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 8.4 - Communication facilities  F:............................. V:............................ T:............................","Item",0]
[]
[null,"Prime cost amounts (B9) ","H3",0]
[]
[null,"Clause 9.1 - Responsibility for prime cost amounts","CONT",0]
[]
[null," F:............................. V:............................ T:............................","Item",0]
[]
[null,"Attendance on subcontractors (B10) ","H3",0]
[]
[null,"Clause 10.1 - General attendance   F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 10.2 - Special attendance","CONT",0]
[]
[null," F:............................. V:............................ T:............................","Item",0]
[]
[null,"General (B11) ","H3",0]
[]
[null,"Clause 11.1 - Protection of the works  F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 11.2 - Protection/isolation of existing/sectionally occupied works  F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 11.3 - Security of the works  F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 11.4 - Notice before covering work  F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 11.5 - Disturbance  F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 11.6 - Environmental disturbance  F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 11.7 - Works cleaning and clearing  F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 11.8 - Vermin  F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 11.9 - Overhand work  F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 11.10 - Tenant installations by direct contractors  F:............................. V:............................ T:............................","Item",0]
[]
[null,"Clause 11.11 - Advertising  F:............................. V:............................ T:............................","Item",0]
[]
[null,"Preliminaries schedule (B12) ","H3",0]
[]
[null,"Information for completion of the preliminaries schedule  Information necessary for elections and completion of those clauses contained in the preliminaries schedule which are necessary for tender purposes is given hereunder. Where no information is given it shall mean that no specific requirements are expected or that the clause is not relevant to this specific contract"]
[]
[null,"12.1 - Provisional bills of quantities [2.2]  "]
[]
[null,"12.2 - Availability of construction information [2.3]  "]
[]
[null,"12.3 - Previous work - dimensional accuracy [3.1]"]
[]
[null,"12.4 - Previous work - defects [3.2]"]
[]
[null,"12.5 - Inspection of adjoining properties [3.3]"]
[]
[null,"12.6 - Defined works area [4.1]"]
[]
[null,"12.7 - Handover of site in stages [4.2]"]
[]
[null,"12.8 - Enclosure of the works [4.3]"]
[]
[null,"12.9 - Geotechnical investigation [4.4]"]
[]
[null,"12.10 - Existing premises occupied [4.6]"]
[]
[null,"12.11 - Services - known [4.7]"]
[]
[null,"12.12 - Protection of trees and/or relevant natural features [4.8]"]
[]
[null,"12.13 - Water [8.1]  Option A (by contractor) - Yes  Option B (by employer - free of charge)  - No  "]
[]
[null,"12.14 - Electricity [8.2] Option A (by contractor) - Yes Option B (by employer - free of charge)  - No"]
[]
[null,"12.15 - Ablution and welfare facilities [8.3]  Option A (by contractor) - Yes  Option B (by employer - free of charge)  - No"]
[]
[null,"12.16 - Communication facilities [8.4]"]
[]
[null,"12.17 - Protection of the works [11.1]"]
[]
[null,"12.18 - Protection/isolation of existing/sectionally occupied works [11.2]  "]
[]
[null,"12.19 - Disturbance [11.5]"]
[]
[null,"12.20 - Environmental disturbance [11.6]"]
[]
[null,"Controlling all forms of pollution  The contractor shall be responsible for and take all precautions in controlling by whatever means necessary all forms of pollution emanating from the site during the construction period due inter alia to noise, artificial light, wind-blown sand, dust, deposits of mud, etc",null,0]
[]
[null,"The contractor is to ensure that all roads which border the site and is used by the contractor during the execution of the works are kept clean and free of any dirt or debris caused by the execution of the works",null,0]
[]
[null,"F:............................. V:............................ T:............................","Item",0]
[]
[null,"SECTION  C: SPECIFIC PRELIMINARIES","H2",0]
[]
[null,"Section C Section C contains specific preliminary items which apply to this contract except where N/A (Not Applicable) appears against an item",null,0]
[]
[null,"The warranty will not be enforced if the work is damaged by defects in the execution of the works, in which case the responsibility for replacement shall rest entirely with the contractor  F:............................. V:............................ T:............................","Item",0]
[]
[null,"Overtime  Should overtime be required to be worked for any reason whatsoever, the cost of such overtime is to be borne by the contractor unless the principal agent has specifically authorised, prior to execution thereof, that costs for such overtime are to be borne by the employer  F:............................. V:............................ T:............................","Item",0]
[]
[null,"Co-operation of the contractor for cost management  It is specifically agreed that the contractor accepts the obligation of assisting the principal agent in implementing proper cost management. The contractor will be advised by the principal agent of all cost management procedures which will be implemented to ensure that the contract value does not exceed the budget  F:............................. V:............................ T:............................","Item",0]
[]
[null,"Overloading  The contractor shall take all necessary steps to ensure that no damage occurs due to overloading of any portion of the works or temporary works eg scaffolding, etc. The contractor shall submit details of his proposed loading, storage, plant erection, etc to the principal agent for approval prior to proceeding with such loading, storing or erecting and shall comply with and pay for the principal agent's requirements in connection with the provision of temporary support work, etc. Any damage caused to the works by overloading shall be made good by the contractor at his sole expense  F:............................. V:............................ T:............................","Item",0]
[]
[null,"Propping of floors below  The contractor is advised that propping of floors below may be required if he wishes to use any areas of completed suspended reinforced concrete slabs for vehicle access, storage of materials and goods and location of plant, scaffolding, etc. The location of these areas and any necessary propping shall be approved by the principal agent and the cost thereof shall be borne by the contractor  F:............................. V:............................ T:............................","Item",0]
[]
[null,"Testing of flat roof waterproofing for watertightness  Flat roof waterproof areas shall be prepared with small sand dykes around them of a size and enclosing an area approved by the principal agent, flooded with water and kept \"ponded\" for at least forty (40) hours as a test to ensure the watertightness of the waterproofing and before any further construction work is carried out above the waterproofing  F:............................. V:............................ T:............................","Item",0]
[]
[null,"The contractor is to submit to the principal agent on an annual basis a schedule of spend, split into vendors engaged as subcontractors and suppliers indicating their BBBEE rating including proof of the said rating  F:............................. V:............................ T:............................","Item",0]
[]
[null,"Advertising rights  The employer may elect to contract with advertising agencies for the erection of advertising hoardings, banners, wraps or the like for the duration of the contract. The contractor shall not prevent such an arrangement and will assist in the facilitation of same. Position and type of advertising structure to be agreed with the principal agent so as not to hinder the contractor in meeting the obligations under this agreement  F:............................. V:............................ T:............................","Item",0]
[]
[null,"Confidentiality  The contractor undertakes to maintain in confidence any and all information regarding this project and shall obtain appropriate similar undertakings from all subcontractors and suppliers. Such information shall not be used in any way except in connection with the execution of the works  No information regarding this project shall be published or disclosed without the prior written consent of the employer  F:............................. V:............................ T:............................","Item",0]
[]
[null,"Media releases  All rights of publication of articles in the media, together with any advertising relating thereto or in any way connected with this project, shall vest with the employer  The contractor together with his subcontractors shall not, without the prior written consent of the employer, cause any statement or advertisement connected with this project to be printed, screened or aired by the media  F:............................. V:............................ T:............................","Item",0]
[]
[null,"SUMMARY OF CATEGORIES","H3",0]
[]
[null,"Category : Fixed   R........................................  Category : Value   R........................................  Category : Time    R........................................",null,0]
[]
[{"$nulls":3},0]
[]
[null,"SECTION NO. 2","H1",0]
[]
[null,"BILL NO. 1 ","H1",0]
[]
[null,"DEMOLITIONS AND ALTERATIONS","H1",0]
[]
[null,"PREAMBLES","H2",0]
[]
[null,"The tenderer is referred to the relevant clauses in the Model Preambles for Trades (2008 Edition) as issued by the Association of South African Quantity Surveyors before pricing this bill",null,0]
[]
[null,"SUPPLEMENTARY PREAMBLES","H2",0]
[]
[null,"Supplementary preamble items described in Bill No. 1, shall equally apply to this Bill.",null,0]
[]
[null,"Existing structures","H3",0]
[]
[null,"In taking down and removing existing work, the utmost care shall be taken to prevent any structural or other damage to the remaining portions on the building and the Contractor shall provide all shoring, needling, strutting, etc. to ensure the stability of all structures during the alteration work, Any damage to the structure and/or building as well as the rectification of same will be for the contractor's account",null,0]
[]
[null,"Services","H3",0]
[]
[null,"Special care shall be exercised during the progress of the work to ensure that electrical installation, water supply pipes, telephone and other services which may be encountered are not interfered with and notice shall be given to the Representative/Agent if any disconnection or alterations become necessary.",null,0]
[]
[null,"Dust and noise","H3",0]
[]
[null,"The Contractor is to take all necessary precautions to the satisfaction of the Representative/Agent to prevent any nuisance from the dust and /or noise whilst carrying out the work.",null,0]
[]
[null,"Disposal of debris","H3",0]
[]
[null,"The Contractor shall be responsible for the removal from site of all materials, debris and rubbish resulting from the work which removal is deemed to be included in the rates unless otherwise stated.",null,0]
[]
[null,"Rates for taking out and removing doors and frames shall include for removing door stops, cabin hooks, etc and making good floor and wall finishes to match existing",null,0]
[]
[null,"Making good of finishes shall include making good of the brick and concrete surfaces onto which the new finishes are applied, where necessary",null,0]
[]
[null,"Temporary support to openings through existing walls","H3",0]
[]
[null,"Making openings, altering openings in existing walls and removing lintels above existing openings shall be done with the utmost care to prevent any structural damage. All necessary supports, propping, shoring, needling, strutting, turning pieces, etc. to walls openings is deemed to be included in the contractor's rates.",null,0]
[]
[null,"Electrical and Mechanical","H3",0]
[]
[null,"Where items include for taking down electrical and mechanical fittings the disconnection and making safe electrically is deemed to be included.",null,0]
[]
[null,"REMOVAL OF EXISTING WORK","H2",0]
[]
[null,"Taking down and removing roofs, floors, panelling, ceilings, partitions, etc","H3",0]
[]
[null,"Pitched concrete tile roof including roof covering, timber trusses and purlins, ceilings and cornices, eaves soffit covering, fascias, barge boards, gutters and rainwater pipes - At Merebank Station","No",1]
[]
[null,"Taking down and removing roofs, floors, panelling, ceilings, partitions, etc","H3",0]
[]
[null,"Roof sheeting from structural steel support structure including damaged fascia and barge boards","m2",1766]
[]
[null,"Acoustic tile suspended ceilings including suspension grid, hangers, etc","m2",2075]
[]
[null,"Taking out and removing doors, windows, etc including thresholds, sills, etc and building up openings in brick walls including making good face brickwork on one side and cement plaster on other side (making good paintwork elsewhere)","H3",0]
[]
[null,"Timber doors, size  813 x 2032mm ","No",97]
[]
[null,"Timber doors, size  1605 x 2032mm ","No",11]
[]
[null,"Taking out/off and removing metalwork","H3",0]
[]
[null,"Roller shutter doors, size  1530 x 2500mm ","No",1]
[]
[null,"Roller shutter doors, size  1800 x 2500mm ","No",8]
[]
[null,"Roller shutter doors, size  2350 x 2500mm ","No",30]
[]
[null,"Hacking up/off and removing floor tile and wall finishes, including removing mortar bed or backing from concrete or brickwork and preparing surfaces for new screed, plaster, tile finishes, etc","H3",0]
[]
[null,"Ceramic tile and preparing screed to receive new floor coverings ","m2",1739]
[]
[null,"Taking  out and removing piping, sanitary fittings, etc including disconnecting  piping  from fittings  and  making good floor and wall finishes (making good tiling and paintwork elsewhere)","H3",0]
[]
[null,"Vitreous china wash hand basin","No",22]
[]
[null,"Vitreous china WC pan with cistern","No",28]
[]
[null,"Taking out/off and removing sundry metalwork","H3",0]
[]
[null,"Galvanised rainwater goods downpipes","m",321]
[]
[null,"Steel gutters ","m",422]
[]
[null,"PREPARATORY WORK TO EXISTING SURFACES","H2",0]
[]
[null,"Remove all loose paint, surface contaminants, friable materials. Remove any mould release agent using clean water, leaving surface clean, dry and dust free. Concrete soffits to be painted, rippel paint texture. 15mm smooth plaster to underside of soffit & painted. Prime surface with one coat professional plaster primer with an overcoating time of 18 hours and finish with two coats of matt paint with an overcoating time of 4 hours. All in strict specifications as per data sheets which may be provided on request, in accordance with preferred manufacturers ","m2",2042]
[]
[null,"MAKING GOOD OF FINISHES ETC","H2",0]
[]
[null,"Making good plaster","H3",0]
[]
[null,"Wall plaster in patches","m2",2224]
[]
[null,"BUDGETARY ALLOWANCES","H2",0]
[]
[null,"Provide a budgetary amount of R150 000,00(One Hundred and Fifty Thousand Rand) for the pressure washing of facebrick walls at Merebank Station .","Item",1,{"v":150000,"d":"150,000.00"},{"v":150000,"d":"R150,000.00"}]
[]
[{"$nulls":3},0]
[]
[null,"SECTION NO. 2","H1",0]
[]
[null,"BILL NO. 2 ","H1",0]
[]
[null,"ROOF COVERINGS","H1",0]
[]
[null,"PREAMBLES","H2",0]
[]
[null,"The tenderer is referred to the relevant clauses in the Model Preambles for Trades (2008 Edition) as issued by the Association of South African Quantity Surveyors before pricing this bill",null,0]
[]
[null,"SUPPLEMENTARY PREAMBLES","H2",0]
[]
[null,"Supplementary preamble items described in Bill No. 1, shall equally apply to this bill.",null,0]
[]
[null,"ROOF SHEETING","H2",0]
[]
[null,"Concealed Fix interlocking 0,58mm thick heavy industrial Z275 spelter galvanised steel sheeting with Chromadek, ColorPlus, Colourbond or Globalcoat finish to one side and Grey other side and accessories, fixed to steel purlins using SL 700 approved clips and fasteners. Cover width 700mm. High wind - 120km/h plus - loading to be considered with installation and fixing must be in accordance with manufacturer's recommendations and specifications.","H3",0]
[]
[null,"Roof sheeting pitch no exceeding 18 degrees","m2",1032]
[]
[null,"ROOF AND WALL INSULATION","H2",0]
[]
[null,"Heavy industrial grade aluminium foil based insulation","H3",0]
[]
[null,"Insulation laid taut over purlins (at approximately 1600mm centres) and fixed concurrent with roof covering including galvanised steel straining wires","m2",1208]
[]
[{"$nulls":3},0]
[]
[null,"SECTION NO. 2","H1",0]
[]
[null,"BILL NO. 3 ","H1",0]
[]
[null,"CARPENTRY AND JOINERY ","H1",0]
[]
[null,"PREAMBLES","H3",0]
[]
[null,"The tenderer is referred to the relevant clauses in the Model Preambles for Trades (2008 Edition) as issued by the Association of South African Quantity Surveyors before pricing this bill",null,0]
[]
[null,"SUPPLEMENTARY PREAMBLES","H2",0]
[]
[null,"Supplementary preamble items described in Bill No. 1, shall equally apply to this bill.",null,0]
[]
[null,"GENERAL NOTES TO TENDERERS","H2",0]
[]
[null,"General notes, described in Bill No.1, shall equally apply to this Bill.",null,0]
[]
[null,"SUPPLEMENTARY PREAMBLES","H3",0]
[]
[null,"Joinery","H4",0]
[]
[null,"Descriptions of frames shall be deemed to include frames, transoms, mullions, rails, etc.",null,0]
[]
[null,"Descriptions of hardwood joinery shall be deemed to be fixed with hardened steel nails or shot pins to brickwork or concrete.",null,0]
[]
[null,"Fixing","H4",0]
[]
[null,"Items described as nailed shall be deemed to be fixed with hardened steel nails or shot pins to brickwork or concrete",null,0]
[]
[null,"Decorative laminate finish","H4",0]
[]
[null,"Laminate finish shall be glued under pressure. Edge strips shall be butt jointed at junctions with adjacent similar finish ",null,0]
[]
[null,"Timber","H4",0]
[]
[null,"All softwood to be South African Pine",null,0]
[]
[null,"Descriptions","H4",0]
[]
[null,"Items described as \"bolted\" shall be deemed to exclude the bolts and include the holes unless otherwise described.",null,0]
[]
[null,"Where the fixing of members is not stated it shall mean the nailing of one timber member to another.",null,0]
[]
[null,"The term \"planted on\" shall mean the nailing of one timber member to another",null,0]
[]
[null,"The term \"screwed on\" shall mean the countersunk screwing of one timber member to another.",null,0]
[]
[null,"The term \"screwed on and pelleted\" shall mean the screwing of one timber member to another with the heads of screw sunk and pelleted.",null,0]
[]
[null,"The term \"plugged\" shall mean the countersunk screwing of a timber member to and including plastic plugs in brickwork or concrete.",null,0]
[]
[null,"The term \"plugged and pelleted\" shall mean the screwing of a timber member to and including plastic plugs in brickwork or concrete with heads of screw sunk and pelleted.",null,0]
[]
[null,"Shelving, etc. described as screwed to steel must be fixed from underside and prices are to include for countersunk drilling through the steel for screw fixing.",null,0]
[]
[null,"Descriptions of floors, ceilings, joinery, etc. shall be deemed to include for all square cutting",null,0]
[]
[null,"Descriptions of items given in linea metre shall be deemed to include for mitres, stopped ends, fitted intersections, etc.",null,0]
[]
[null,"Descriptions of rounded angles, rebates, grooves, chamfers, moulded edges, etc. shall be deemed to include for angles, ends, etc.",null,0]
[]
[null,"ROOFS, ETC","H2",0]
[]
[null,"Plate nailed timber roof truss construction","H3",0]
[]
[null,"The following is applicable in respect of roof trusses:All timber to be sawn softwood in accordance with V4 or M4 as defined in SABS 563 or SABS 1245.Metal connector plates shall have a minimum yield strength of 228 MPa and a minimum ultimate tensile strength of 330 Mpa with hot-dip galvanised finish.All joints to be close fitted butt joints.Trusses shall be designed by a registered supplier of prefabricated trusses who shall issue an Engineers Certificate upon completion of the installation. The dimensions in the descriptions of the trusses are nominal and actual measurements are to be obtained on site before design or fabrication commences.Tenderers must study the roof plan and sections as attached to the back of these bills of quantities and must obtain prices from a qualified and registered roof truss supplier as no claims in this regard will be entertained.",null,0]
[]
[null,"Sawn softwood","H3",0]
[]
[null,"Design, take delivery, temporary store, hoist in position and erect plate nailed termite treated timber roof trusses, purlins, gangboarding, temporary and permanent bracing, etc (measured on plan). -  to Merebank Station","m2",258]
[]
[null,"FASCIAS AND BARGE BOARDS","H3",0]
[]
[null,"15 x 225mm Fascia board countersunk screwed to roof timbers (elsewhere) with two brass screws at maximum 754mm centres and jointed with and including standard aluminium halfround cover strips at all","m",653]
[]
[null,"DOORS ETC","H2",0]
[]
[null,"Heavy duty anti bandit timber door, with gms (coastal) or ms (inland) pressed metal frame to suite door & wall. Including 300x300mm glass viewing panels with aluminium frames and rubber gaskets.","H3",0]
[]
[null,"900 x 2032 x 44mm aluminium framed solid door - TP-01","No",8]
[]
[null,"900 x 2032 x 44mm aluminium framed solid door - TP-04","No",5]
[]
[null,"Semi solid timber door sides and concealed edges to suit opening, door to be fitted with 3 x hinges per leaf all to specialist details. Colour of the door and frame to architect's specialist.","H3",0]
[]
[null,"900 x 2100mm aluminium framed solid door - TP-02","No",13]
[]
[null,"900 x 2100mm aluminium framed solid door - TP-06","No",49]
[]
[null,"900 x 2100mm aluminium framed solid door - TP-07","No",5]
[]
[null,"Solid timber door sides and concealed edges to suit opening, door to be fitted with 3 x hinges per leaf all to specialist details. Colour of the door and frame to architect's specialist.","H3",0]
[]
[null,"900 x 2100mm steel framed (elsewhere) solid door - TP-03","No",52]
[]
[null,"FIRE DOORS ETC","H2",0]
[]
[null,"Class \"B\" 2 hour fire rated solid hardwood double door, all purpose made, steel frame to suite door & wall. Primed & painted with 2 coats","H3",0]
[]
[null,"1800 X 2100mm aluminium framed solid door - TP-01","No",7]
[]
[{"$nulls":3},0]
[]
[null,"SECTION NO.2","H1",0]
[]
[null,"BILL NO. 4","H1",0]
[]
[null,"CEILINGS, PARTITIONS AND ACCESS FLOORING","H1",0]
[]
[null,"PREAMBLES","H2",0]
[]
[null,"The tenderer is referred to the relevant clauses in the Model Preambles for Trades (2008 Edition) as issued by the Association of South African Quantity Surveyors before pricing this bill",null,0]
[]
[null,"SUPPLEMENTARY PREAMBLES","H2",0]
[]
[null,"Note:","H3",0]
[]
[null,"Electrical  light  fittings, diffusers, panels, etc generally are \"lay  in\"  units  of  the  same dimensions as the suspension grid described  and  allowance  must  be  made  accordingly  for their support  inclusive  of any flexibility insetting out that may be required (ceiling panels have not been deducted and pricing is to take cognisance thereof)",null,0]
[]
[null,"GENERAL NOTES TO TENDERERS","H2",0]
[]
[null,"General notes, described in Section No.1, Bill No.1, shall equally apply to this Bill.",null,0]
[]
[null,"CEILINGS ETC","H2",0]
[]
[null,"SUSPENDED CEILINGS","H2",0]
[]
[null,"9,5mm Flush plaster gypsum or Magna Board ceiling fixed to concealed suspended tee system skimmed. Ceiling grid to be 1200 c/c. Fixed to concealed suspended tee system, skimmed and prepared to receive 2 coats quality pva paint (elsewhere). All in strict accordance with manufactures specification & requirements. ","H3",0]
[]
[null,"Suspended Ceilings ","m2",468]
[]
[null,"12mm Flush plaster gypsum or Magna Board ceiling fixed to concealed suspended tee system skimmed. Ceiling grid to be 1200 c/c. Fixed to concealed suspended tee system, skimmed and prepared to receive 2 coats quality pva paint (elsewhere). All in strict accordance with manufactures specification & requirements.","H3",0]
[]
[null,"Suspended Ceilings ","m2",475]
[]
[null,"12.5mm vinyl faced gypsum ceiling panels, face-covered with white embossed vinyl, size 1200 x 600mm, laid on fire rated cliq system s3 exposed demountable suspension system including galvanised main tees, cross Tees, etc., all suspended with galvanised hangers at centres not exceeding 1200mm, with ceiling perimeter finished with shadowline w-trim plugged at 200mm centres, and all installed to manufacturer's Instructions.   ","H3",0]
[]
[null,"Suspended Ceilings ","m2",1381]
[]
[null,"CEILING INSULATION","H2",0]
[]
[null,"50mm cellulose fibre insulation applied strictly in accordance with the manufacturer's instructions.","m2",1052]
[]
[{"$nulls":3},0]
[]
[null,"SECTION NO.2","H1",0]
[]
[null,"BILL NO. 5 ","H1",0]
[]
[null,"IRONMONGERY","H1",0]
[]
[null,"PREAMBLES","H2",0]
[]
[null,"The tenderer is referred to the relevant clauses in the Model Preambles for Trades (2008 Edition) as issued by the Association of South African Quantity Surveyors before pricing this bill",null,0]
[]
[null,"SUPPLEMENTARY PREAMBLES","H2",0]
[]
[null,"Supplementary preamble items described in Bill No. 1, shall equally apply to this bill.",null,0]
[]
[null,"BUDGETARY ALLOWANCES","H1",0]
[]
[null,"IRONMONGERY FIXED TO DOORS, etc.","H2",0]
[]
[null,"Allow an amount of R22 250,00 (Twenty Two Thousand Two Hundred and Fifty Rand) for the  ironmongery to specialist according to the schedule at Congella Station ","Item",1,{"v":22250,"d":"22,250.00"},{"v":22250,"d":"R22,250.00"}]
[]
[null,"Allow an amount of R40 000,00 (Forty Thousand Rand) for the ironmongery to specialist according to the schedule at Umbilo Station ","Item",1,{"v":40000,"d":"40,000.00"},{"v":40000,"d":"R40,000.00"}]
[]
[null,"Allow an amount of R47 250,00 (Forty Seven Thousand Two Hundred and Fifty Rand) for the ironmongery to specialist according to the schedule at Rossburgh Station ","Item",1,{"v":47250,"d":"47,250.00"},{"v":47250,"d":"R47,250.00"}]
[]
[null,"Allow an amount of R46 250,00 (Forty Six Thousand Two Hundred and Fifty Rand) for the ironmongery to specialist according to the schedule at Merebank Station ","Item",1,{"v":46250,"d":"46,250.00"},{"v":46250,"d":"R46,250.00"}]
[]
[{"$nulls":3},0]
[]
[null,"SECTION NO.2","H1",0]
[]
[null,"BILL NO. 6 ","H1",0]
[]
[null,"METALWORK ","H1",0]
[]
[null,"PREAMBLES","H2",0]
[]
[null,"The tenderer is referred to the relevant clauses in the Model Preambles for Trades (2008 Edition) as issued by the Association of South African Quantity Surveyors before pricing this bill",null,0]
[]
[null,"SUPPLEMENTARY PREAMBLES","H2",0]
[]
[null,"Supplementary preamble items described in Bill No. 1, shall equally apply to this bill.",null,0]
[]
[null,"PRESSED STEEL TRANSFORMER ROOM DOORS AND FRAMES","H2",0]
[]
[null,"Galvanised and epoxy coated m/s steel door sides and concealed edges to suit opening, door to be fitted with 3 x hinges per leaf all to specialist details.","H3",0]
[]
[null,"Door size 900mm x 2100mm - TP-05","No",41]
[]
[null,"STEEL ROLLER SHUTTERS ETC","H2",0]
[]
[null,"Approved roll-up perforated galvanised, sabs 1461, & epoxy coated m/s perforated roller shutter door. Electrically operated with 220 volt hl600 motor with manual override, with 75 x 1.0mm thick galv. Endlocked slats complete with nylon end-locks, 120mm extra-wide tamper proof m/s guides, powder coated ancillary components including door curtain, 4.5mm thick end plates, guide rails, closed shaft, extruded aluminium t-bar with astragal rubber weather seal, & single span (no join) galv. Cover box. Operated with high security key switch. Fixed to brick, concrete or structural steel jambs and structural steel beam over. Contractor to provide cavity of 160mm x 120mm for recessing guides.","H3",0]
[]
[null,"Electrically operated slatted roller shutter for 925 x 1100mm high opening ","No",13]
[]
[null,"Electrically operated slatted roller shutter for 1530 x 2500mm high opening ","No",1]
[]
[null,"Electrically operated slatted roller shutter for 1800x 2500mm high opening","No",8]
[]
[null,"Electrically operated slatted roller shutter for 2350 x 2500mm high opening","No",30]
[]
[null,"PRESSED STEEL DOOR FRAMES ","H2",0]
[]
[null,"Standard single rebate steel frame suitable for one brick wall, with 1 pr. 100mm brass butt hinges. Clean down, prepare and apply 1 coat red oxide. Primer 1 undercoat, 2 coats enamel to developer's approval (elsewhere)","H3",0]
[]
[null,"Single door size frame 813 x 2032 mm high","No",18]
[]
[null,"ALUMINIUM WINDOWS, ETC","H2",0]
[]
[null,"Standard aluminium window frame. Manufactured with approved aluminium sections. Powder coated to Architect's spec. Supplied with glazing (clear glass and opaque glass in bathrooms). Manufacturer to fit galvanised steel lugs to frame, to built into brick wall to spec. (as per schedule)","H3",0]
[]
[null,"Window panel, size 6960 x 2785mm high - Congella (TP-01)","No",1]
[]
[null,"Window panel, size 1160 x 655mm high - Congella (TP-02)","No",3]
[]
[null,"Window panel, size 700 x 1100 mm high - Congella (TP-03)","No",5]
[]
[null,"Window panel, size 600 x 540mm high - Congella (TP-05)","No",30]
[]
[null,"Window panel, size 1680 x 540mm high - Congella (TP-06)","No",2]
[]
[null,"Window panel, size 5800 x 3420mm high - Umbilo (TP-01)","No",2]
[]
[null,"Window panel, size 2030 x 3420mm high - Umbilo (TP-02)","No",2]
[]
[null,"Window panel, size 600 x 2100 mm high - Umbilo (TP-03)","No",1]
[]
[null,"Window panel, size 7300 x 3405mm high - Umbilo (TP-05)","No",1]
[]
[null,"Window panel, size 925 x 1100mm high - Umbilo (TP-06)","No",9]
[]
[null,"Window panel, size 700 x 1100mm high - Rossburgh (TP-01)","No",12]
[]
[null,"Window panel, size 1800 x 540mm high - Rossburgh (TP-02)","No",2]
[]
[null,"Window panel, size 1200 x 540mm high - Rossburgh (TP-03)","No",2]
[]
[null,"Window panel, size 3000 x 1500mm high - Rossburgh (TP-04)","No",18]
[]
[null,"Window panel, size 1515 x 1500mm high - Rossburgh (TP-05)","No",18]
[]
[null,"Window panel, size 600 x 600mm high - Rossburgh (TP-06)","No",33]
[]
[null,"Window panel, size 600 x 1100mm high - Rossburgh (TP-07)","No",6]
[]
[null,"Window panel, size 1855 x 1100 mm high - Rossburgh (TP-08)","No",22]
[]
[null,"Window panel, size 1855 x 1500mm high - Rossburgh (TP-09)","No",8]
[]
[null,"Window panel, size 10760 x 1000mm high - Merebank (TP-01)","No",4]
[]
[null,"Window panel, size 700 x 1100mm high - Merebank (TP-02)","No",3]
[]
[null,"Window panel, size 560 x 540mm high - Merebank (TP-04)","No",14]
[]
[null,"Window panel, size 705 x 700mm high - Merebank (TP-05)","No",14]
[]
[null,"Window panel, size 1600 x 1195mm high - Merebank (TP-06)","No",2]
[]
[null,"ALUMINIUM DOORS, ETC","H2",0]
[]
[null,"Standard aluminium window frame. Manufactured with approved aluminium sections. Powder coated to Architect's spec. Supplied with glazing (clear glass and opaque glass in bathrooms). Manufacturer to fit galvanised steel lugs to frame, to built into brick wall to spec. (as per schedule)","H3",0]
[]
[null,"Door size 900 x 2145mm high (TP-09)","No",1]
[]
[null,"Door size 1600 x 2145mm high (TP-10)","No",4]
[]
[{"$nulls":3},0]
[]
[null,"SECTION NO. 2","H1",0]
[]
[null,"BILL NO.7","H1",0]
[]
[null,"TILING","H1",0]
[]
[null,"PREAMBLES ","H2",0]
[]
[null,"The tenderer is referred to the relevant clauses in the Model Preambles for Trades (2008 Edition) as issued by the Association of South African Quantity Surveyors before pricing this bill",null,0]
[]
[null,"SUPPLEMENTARY PREAMBLES ","H2",0]
[]
[null,"Descriptions Unless described as \"fixed with adhesive to plaster (plaster elsewhere)\" descriptions of tiling on brick or concrete walls, columns, etc shall be deemed to include 1:4 cement plaster backing and descriptions of tiling on concrete floors etc shall be deemed to include 1:3 plaster bedding.",null,0]
[]
[null,"FLOOR TILING","H2",0]
[]
[null,"Full bodied porcelain tiles, size 600 x 600mm x 10mm (P.C allowance of R 150.00/m2 excludes V.A.T. but includes delivery to site), min R9 preferably R10 slip rated fixed to internal floor screed with tile adhesive mixed with bonding liquid in lieu of water with diagonal joints continuous in both directions and grouted with 3mm tile grout, excess grout on the surface to be cleaned with water as work proceeds.","H3",0]
[]
[null,"On floors ","m2",958]
[]
[null,"100mm high skirting","m",1258]
[]
[{"$nulls":3},0]
[]
[null,"SECTION NO. 2","H1",0]
[]
[null,"BILL NO. 8","H1",0]
[]
[null,"PLUMBING AND DRAINAGE (PROVISIONAL)","H1",0]
[]
[null,"PREAMBLES","H2",0]
[]
[null,"The tenderer is referred to the relevant clauses in the Model Preambles for Trades (2008 Edition) as issued by the Association of South African Quantity Surveyors before pricing this bill",null,0]
[]
[null,"Note:","H4",0]
[]
[null,"All glazed ceramic sanitaryware to comply with SABS 497  All stainless steelware for medical institutions to comply with SABS 497  Stainless steel sinks to comply with SABS 907  Stainless steel washtroughs to comply with SABS 906  Cisterns to comply with SABS 821 and fitments to SABS 1509  All taps to comply to SABS 226 ",null,0]
[]
[null,"RAINWATER GOODS","H2",0]
[]
[null,"225 x 225mm PVC gutters including rivet-fixed mitres and end caps internally sealed using Silicon Mastic, hung by hangers with downpipes (elsewhere specified). Install strictly to manufacturer’s specifications. Profile, type and finish all to Architect's approval","H3",0]
[]
[null,"PVC gutters with 20mm overlapping joints sealed with and including bitumen impregnated foam plastic joint sealing strip and riveted at 20mm centres","m",652]
[]
[null,"80mm PVC down pipe fixed to brick wall including brackets","m",321]
[]
[null,"Extra over eaves gutter for offset","No",107]
[]
[null,"Extra over eaves gutter for outlet","No",107]
[]
[null,"Extra over eaves gutter for stopped end","No",107]
[]
[null,"Extra over for shoe ","No",107]
[]
[null,"SANITARY FITTINGS ","H2",0]
[]
[null,"Refer to sanitary schedule drawing for full description of abbreviations ",null,0]
[]
[null,"Approved  ","H3",0]
[]
[null,"Vitreous china close coupled washdown suite colour: white, comprising 90Deg. outlet open rim pan and matching 6 litre top dual flush cistern including lid and fitments, with thermoset seat. ","No",35]
[]
[null,"Ceramic fire clay drop-in vanity basin, colour: white,size 595 x 455mm including chain stay hole fitted into opening in vanity top (elsewhere specified) and sealed with silicone sealant where basin rim meets vanity top. ","No",29]
[]
[null,"WASTE UNIONS, TRAPS ETC.","H2",0]
[]
[null,"The following sanitary fittings to SABS specifications, etc.","H3",0]
[]
[null,"Approved ","H3",0]
[]
[null,"32mm chrome plated bottle trap ","No",29]
[]
[null,"TAPS, FLUSH VALVES, ETC ","H2",0]
[]
[null,"Approved ","H3",0]
[]
[null,"Selene basin mixer including valves","No",29]
[]
[null,"TESTING","H2",0]
[]
[null,"Testing water pipe system","Item",1]
[]
[null,"SANITARY PLUMBING ","H2",0]
[]
[null,"Sewer and drainage pipes and fittings shall be through Solid wall Class 34 uPVC socketed soil piping in according to SABS 791, jointed and sealed with butyl rubber rings Soil, waste and vent pipes and fittings shall be according to SABS 967 and solvent jointed  Cold water supply pressure pipes and fittings shall be according to SABS 966 and jointed by means of the \"Lyng\" type jointing system  Pipes shall be fixed and jointed according to SABS 0112","H2",0]
[]
[null,"Class 34 uPVC Pipe","H3",0]
[]
[null,"50mm pipes ","m",122]
[]
[null,"110mm pipes ","m",141]
[]
[null,"160mm pipes ","m",300]
[]
[null,"Class 34 uPVC FITTINGS","H3",0]
[]
[null,"50mm 90 degree Bend ","No",18]
[]
[null,"50mm 45 degree Bend","No",13]
[]
[null,"50mm Equal Access junction","No",56]
[]
[null,"110mm 45 degree Bend","No",15]
[]
[null,"110mm pan connector","No",78]
[]
[null,"110mm 90 degree Bend","No",6]
[]
[null,"110mm 90 degree access Bend","No",6]
[]
[null,"110mm diameter - 50mm diameter junction","No",36]
[]
[null,"110mm Equal Access junction","No",6]
[]
[null,"160mm diameter- 110mm diameter junction","No",31]
[]
[null,"160mm diameter 90 Deg Bend","No",60]
[]
[null,"Pipe Hangers - Anchor, Treaded Rod & Hanger","H3",0]
[]
[null,"50mm","No",9]
[]
[null,"110mm","No",9]
[]
[null,"WATER SUPPLY","H2",0]
[]
[null,"COLD WATER RETICULATION","H2",0]
[]
[null,"Replace defective pipe sections and fittings","H3",0]
[]
[null,"PEX Piping","H3",0]
[]
[null,"15mm Diameter pipe. ","m",246]
[]
[null,"22mm Diameter pipe. ","m",175]
[]
[null,"Extra over PEX pipes for fittings:","H3",0]
[]
[null,"15mm elbow.","No",153]
[]
[null,"22mm elbow. ","No",89]
[]
[null,"22mm equal Tee","No",115]
[]
[null,"22-15 mm Reducer","No",116]
[]
[null,"Plastic Pipe Compression Fittings And Valves","H3",0]
[]
[null,"15mm elbow.","No",52]
[]
[null,"22mm Isolation Valve. ","No",35]
[]
[null,"22mm Strainer Valve","No",35]
[]
[null,"Pipe Hangers - Anchor, Treaded Rod & Hanger","H3",0]
[]
[null,"15mm Diameter pipe. ","No",115]
[]
[null,"22mm Diameter pipe. ","No",65]
[]
[null,"Heavy brown paper loosely wrapped around pipe as sheath for expansion.","H3",0]
[]
[null,"15 - 22mm Diameter pipe. ","m",216]
[]
[null,"Provision For Pipework Chasing and Making Good After","m",196]
[]
[{"$nulls":3},0]
[]
[null,"SECTION NO.2","H1",0]
[]
[null,"BILL NO. 9","H1",0]
[]
[null,"PAINTWORK","H1",0]
[]
[null,"PREAMBLES","H2",0]
[]
[null,"The tenderer is referred to the relevant clauses in the Model Preambles for Trades (2008 Edition) as issued by the Association of South African Quantity Surveyors before pricing this bill",null,0]
[]
[null,"SUPPLEMENTARY PREAMBLES","H2",0]
[]
[null,"Supplementary preamble items described in Bill No. 1, shall equally apply to this bill.",null,0]
[]
[null,"PAINTWORK ETC TO EXISTING WORK","H2",0]
[]
[null,"ON FLOATED PLASTER","H2",0]
[]
[null,"Prepare and apply one coat professional plaster primer and two coats acrylic PVA paint. Colour to Architect and Client Approval","H3",0]
[]
[null,"Plastered walls","m2",3019]
[]
[null,"METAL SURFACES","H2",0]
[]
[null,"Prepare and apply one coat professional plaster primer, universal undercoat and two coats super enamel. Colour to Architect and Client Approval ","H3",0]
[]
[null,"On doors frames","m2",32]
[]
[null,"ON WOOD","H2",0]
[]
[null,"Prepare and paint three coats clear varnish:","H3",0]
[]
[null,"On doors  ","m2",563]
[]
[null,"SMOOTH CONCRETE","H2",0]
[]
[null,"One coat alkali resistant primer and two coats superior quality acrylic emulsion paint for interior and exterior use. Colour to Architect and Client Approval","H3",0]
[]
[null,"Soffits of slab ","m2",577]
[]
[null,"PAINTWORK ETC TO NEW WORK","H2",0]
[]
[null,"ON FLOATED PLASTER","H2",0]
[]
[null,"Prepare and apply one coat professional plaster primer and two coats acrylic PVA paint. Colour to Architect and Client Approval","H3",0]
[]
[null,"Plastered walls","m2",3831]
[]
[null,"ON PLASTER BOARD","H2",0]
[]
[null,"Prepare and apply one coat primer and two coats internal paint with mat finish. Colour to Architect and Client Approval","H3",0]
[]
[null,"On internal ceilings and cornices  ","m2",475]
[]
[{"$nulls":3},0]
[]
[null,"SECTION NO. 2","H1",0]
[]
[null,"BILL NO. 10","H1",0]
[]
[null,"PROVISIONAL SUMS","H1",0]
[]
[null,"Note","H3",0]
[]
[null,"The items described hereunder cover work which is not fully defined at tender date and which is intended to be executed by the contractor and/or his subcontractors. The amounts shown shall be used as directed by the principal agent and shall be deducted in all or in part if not required.",null,0]
[]
[null,"STATION FIXED FURNITURE","H3",0]
[]
[null,"Allow an amount of R75 000,00 (Seventy Five Thousand Rand) for the installation of fixed furniture at Congella Station","Item",1,{"v":75000,"d":"75,000.00"},{"v":75000,"d":"R75,000.00"}]
[]
[null,"Allow an amount of R75 000,00 (Seventy Five Thousand Rand) for the installation of fixed furniture at Umbilo Station","Item",1,{"v":75000,"d":"75,000.00"},{"v":75000,"d":"R75,000.00"}]
[]
[null,"Allow an amount of R100 000,00 (One Hundred Thousand Rand)for the installation of fixed furniture at Rossburgh Station","Item",1,{"v":100000,"d":"100,000.00"},{"v":100000,"d":"R100,000.00"}]
[]
[null,"Allow an amount of R250 000,00 (Two Hundred and Fifty Thousand Rand)for the installation of fixed furniture at Merebank Station","Item",1,{"v":250000,"d":"250,000.00"},{"v":250000,"d":"R250,000.00"}]
[]
[null,"Profit","%IT"]
[]
[null,"Attendance","%IT"]
[]
[null,"STATION SIGNAGE","H3",0]
[]
[null,"Allow an amount of R40 000,00 (Forty Thousand Rand) for the installation of missing signage at Congella Station","Item",1,{"v":40000,"d":"40,000.00"},{"v":40000,"d":"R40,000.00"}]
[]
[null,"Allow an amount of R40 000,00 (Forty Thousand Rand) for the installation of missing signage at Umbilo Station","Item",1,{"v":40000,"d":"40,000.00"},{"v":40000,"d":"R40,000.00"}]
[]
[null,"Allow an amount of R40 000,00 (Forty Thousand Rand) for the installation of missing signage at Rossburgh Station","Item",1,{"v":40000,"d":"40,000.00"},{"v":40000,"d":"R40,000.00"}]
[]
[null,"Allow an amount of R50 000,00 (Fifty Thousand Rand) for the installation of missing signage at Merebank station","Item",1,{"v":50000,"d":"50,000.00"},{"v":50000,"d":"R50,000.00"}]
[]
[null,"Profit","%IT"]
[]
[null,"Attendance","%IT"]
[]
[null,"COMMUNITY LIAISON OFFICER","H3",0]
[]
[null,"Allow an amount of R90 000,00 (Ninety Thousand Rand) for a Community Liaison Officer at Congella Station","Item",1,{"v":90000,"d":"90,000.00"},{"v":90000,"d":"R90,000.00"}]
[]
[null,"Allow an amount of R90 000,00 (Ninety Thousand Rand) for a Community Liaison Officer at Umbilo Station","Item",1,{"v":90000,"d":"90,000.00"},{"v":90000,"d":"R90,000.00"}]
[]
[null,"Allow an amount of R90 000,00 (Ninety Thousand Rand) for a Community Liaison Officer at Rossburgh Station","Item",1,{"v":90000,"d":"90,000.00"},{"v":90000,"d":"R90,000.00"}]
[]
[null,"Allow an amount of R90 000,00 (Ninety Thousand Rand) for a Community Liaison Officer Merebank Station.","Item",1,{"v":90000,"d":"90,000.00"},{"v":90000,"d":"R90,000.00"}]
[]
[null,"Profit","%IT"]
[]
[null,"PROTECTION SERVICES","H3",0]
[]
[null,"Allow an amount of R200 000,00 (Two Hundred Thousand Rand) for occupation at Congella Station","Item",1,{"v":200000,"d":"200,000.00"},{"v":200000,"d":"R200,000.00"}]
[]
[null,"Allow an amount of R200 000,00 (Two Hundred Thousand Rand) for occupation at Umbilo Station","Item",1,{"v":200000,"d":"200,000.00"},{"v":200000,"d":"R200,000.00"}]
[]
[null,"Allow an amount of R200 000,00 (Two Hundred Thousand Rand) for occupation at Rossburgh Station","Item",1,{"v":200000,"d":"200,000.00"},{"v":200000,"d":"R200,000.00"}]
[]
[null,"Allow an amount of R200 000,00 (Two Hundred Thousand Rand) for occupation at Merebank Station","Item",1,{"v":200000,"d":"200,000.00"},{"v":200000,"d":"R200,000.00"}]
[]
[null,"Profit","%IT"]
[]
[null,"Attendance","%IT"]
[]
[{"$nulls":3},0]
[]
[null,"SECTION NO.2","H1",0]
[]
[null,"BILL NO.11","H1",0]
[]
[null,"BUDGETARY ALLOWANCES","H1",0]
[]
[null,"Note","H3",0]
[]
[null,"The items described hereunder cover work which is not fully defined at tender date and which is intended to be executed by the contractor and/or his subcontractors. The amounts shown shall be used as directed by the principal agent and shall be deducted in all or in part if not required.",null,0]
[]
[null,"BINS & BENCHES","H3",0]
[]
[null,"Allow an amount of R190 000,00 (One Hundred and Ninety Thousand Rand) for bins and benches at Congella Station","Item",1,{"v":190000,"d":"190,000.00"},{"v":190000,"d":"R190,000.00"}]
[]
[null,"Allow an amount of R25 000,00 (Twenty Five Thousand Rand) for bins and benches at Umbilo Station","Item",1,{"v":25000,"d":"25,000.00"},{"v":25000,"d":"R25,000.00"}]
[]
[null,"Allow an amount of R109 000,00 (One Hundred and Nine Thousand Rand) for bins and benches at Rossburgh Station","Item",1,{"v":109000,"d":"109,000.00"},{"v":109000,"d":"R109,000.00"}]
[]
[null,"Allow an amount of R20 000,00 (Twenty Thousand Rand) for bins and benches at Merebank Station","Item",1,{"v":20000,"d":"20,000.00"},{"v":20000,"d":"R20,000.00"}]
[]
[null,"Profit","%IT"]
[]
[null,"RESURFACING","H3",0]
[]
[null,"Allow an amount of R25 000,00 (Twenty Five Thousand Rand) for the resurfacing on the platforms at Congella Station ","Item",1,{"v":25000,"d":"25,000.00"},{"v":25000,"d":"R25,000.00"}]
[]
[null,"Allow an amount of R25 000,00 (Twenty Five Thousand Rand) for the resurfacing on the platforms at Umbilo Station ","Item",1,{"v":25000,"d":"25,000.00"},{"v":25000,"d":"R25,000.00"}]
[]
[null,"Allow an amount of R50 000,00 (Fifty Thousand Rand) for the resurfacing on the platforms at Rossburgh Station ","Item",1,{"v":50000,"d":"50,000.00"},{"v":50000,"d":"R50,000.00"}]
[]
[null,"Allow an amount of R35 000,00 (Thirty Five Thousand Rand) for repairs to the stormwater drain by the entrance at Merebank Station ","Item",1,{"v":35000,"d":"35,000.00"},{"v":35000,"d":"R35,000.00"}]
[]
[null,"Profit","%IT"]
[]
[{"$nulls":3},0]
[]
[null,"Alterations and Renovations ","Page",27,0]
[]
[null,"Roof Coverings","Page",28,0]
[]
[null,"Carpentry and Joinery ","Page",32,0]
[]
[null,"Ceilings, Partitioning and access flooring","Page",34,0]
[]
[null,"Ironmongery","Page",35,0]
[]
[null,"Metalwork","Page",39,0]
[]
[null,"Tiling","Page",40,0]
[]
[null,"Plumbing and Drainage (Provisional)","Page",45,0]
[]
[null,"Paintwork ","Page",47,0]
[]
[null,"Provisional Sums","Page",50,0]
[]
[null,"Budgetary Allowances","Page",52,0]
[]
[null,"SECTION NO. 3","H1",0]
[]
[null,"BILL NO. 1 ","H1",0]
[]
[null,"ELECTRICAL INSTALLATION","H1",0]
[]
[null,"LOW VOLTAGE ","H2",0]
[]
[null,"DISCONNECTION/ REMOVAL OF REDUNDANT ELECTRICAL EQUIPMENT","H2",0]
[]
[null,"The following equipment shall be isolated, disconnected, removed and handed over to the Employer's","H3",0]
[]
[null,"CONGELLA STATION","H3",0]
[]
[null,"Decommissioning and stripping of existing electrical installations including cables, conductors, luminiares, control devices, DB's, etc in the existing building.","Item",1,{"v":30000,"d":"30,000.00"},{"v":30000,"d":"R30,000.00"}]
[]
[null,"UMBILO STATION ","H3",0]
[]
[null,"Decommissioning and stripping of existing electrical installations including cables, conductors, luminiares, control devices, DB's, etc in the existing building.","Item",1,{"v":5000,"d":"5,000.00"},{"v":5000,"d":"R5,000.00"}]
[]
[null,"ROSSBURGH STATION ","H3",0]
[]
[null,"Decommissioning and stripping of existing electrical installations including cables, conductors, luminiares, control devices, DB's, etc in the existing building.","Item",1,{"v":80000,"d":"80,000.00"},{"v":80000,"d":"R80,000.00"}]
[]
[null,"MEREBANK STATION ","H3",0]
[]
[null,"Decommissioning and stripping of existing electrical installations including cables, conductors, luminiares, control devices, DB's, etc in the existing building.","Item",1,{"v":30000,"d":"30,000.00"},{"v":30000,"d":"R30,000.00"}]
[]
[null,"LV SWITCHGEAR DBs and LV Switchgear ","H2",0]
[]
[null,"Manufacture, deliver to site, install, commission, test kiosks, distribution boards as per specification and single line diagram, to be housed in electrical. All electrical panels shall be stainless steel material, rates to include powder coated, busbars and drilling, busbar connections internal wiring etc. Refer to single line diagram for electrical panel colour","H3",0]
[]
[null,"CONGELLA STATION","H4",0]
[]
[null,"Kiosk 1","No",1]
[]
[null,"Kiosk 2","No",1]
[]
[null,"DB - 1","No",4]
[]
[null,"DB - 2","No",7]
[]
[null,"Surface mounted UT4 IP65 Box complete with 32A, 1-pole isolator,  3x 10A circuit breakers with complete with busbars","No",12]
[]
[null,"UMBILO STATION","H4",0]
[]
[null,"Sub-DB A1","No",1]
[]
[null,"Sub-DB A2","No",1]
[]
[null,"Surface mounted UT4 IP65 Box complete with 32A, 1-pole isolator,  3x 10A circuit breakers with complete with busbars","No",6]
[]
[null,"ROSSBURGH STATION","H4",0]
[]
[null,"Kiosk AE","No",1]
[]
[null,"Kiosk 1","No",1]
[]
[null,"Kiosk 2","No",2]
[]
[null,"DB - 1 & 2","No",2]
[]
[null,"Surface mounted UT4 IP65 Box complete with 32A, 1-pole isolator,  3x 10A circuit breakers with complete with busbars","No",1]
[]
[null,"Kiosk concrete plinth for Kiosk AE. Refer to attached kiosk drawings - dimenstions are 950mmx 650mmx 150mm and must be 25Mpa. Rate to include removing existing kiosk and slap , clean up, prepare for new slab and construction of new concrete slab","SUM",1]
[]
[null,"MEREBANK STATION","H4",0]
[]
[null,"DB - 1","No",1]
[]
[null,"DB - 2","No",1]
[]
[null,"DB - 3","No",1]
[]
[null,"Surface mounted UT4 IP65 Box complete with 32A, 1-pole isolator,  3x 10A circuit breakers with complete with busbars","No",6]
[]
[null,"CABLES AND CONDUCTORS","H2",0]
[]
[null,"Supply, deliver to site cables and conductors as specified. Install, rack, strap and testing of cables as per specification including clamps, ties and cable numbering system","H3",0]
[]
[null,"2,5mm conductors (mixed colours - live, neutral and earth)","m",13200]
[]
[null,"2.5 mm² 2c 600/1000V PVC/SWA/PVC ECC Cu Cable ","m",1201]
[]
[null,"2.5 mm² 4c 600/1000V PVC/SWA/PVC ECC Cu Cable ","m",400]
[]
[null,"4,0mm conductors (mixed colours - live, neutral and earth)","m",7800]
[]
[null,"10 mm² 4c 600/1000V PVC/SWA/PVC ECC Cu Cable ","m",780]
[]
[null,"16mm² 4c 600/1000V PVC/SWA/PVC ECC Cu Cable ","m",10]
[]
[null,"70 mm² 4c 600/1000V PVC/SWA/PVC ECC Cu Cable ","m",460]
[]
[null,"CABLES AND CONDUCTORS","H2",0]
[]
[null,"Termination of cables shall include supply installation and testing of the glands with corrossion  guard , making-off the cable, lugs, and fitting the gland to the board gland plate, switchgear or equipment and final connection of cable tails into board or terminals.  Include for Reducing Glands and shrouds where applicable. NB:  IP65 Glands are to be used where applicable. ","H3",0]
[]
[null,"2,5mm² 4c 600/1000V PVC/SWA/PVC ECC Cu Cable","No",90]
[]
[null,"10 mm² 4c 600/1000V PVC/SWA/PVC ECC Cu Cable ","No",22]
[]
[null,"16mm² 4c 600/1000V PVC/SWA/PVC ECC Cu Cable ","No",2]
[]
[null,"70mm² 4c 600/1000V PVC/SWA/PVC ECC Cu Cable ","No",12]
[]
[null,"25mm PVC Conduit including all necessary accessories. Rate to include chasing wall for conduit in the wall, close wall and make good.","m",2060]
[]
[null,"25mm steel Conduit including all necessary accessories. Rate to include chasing wall for conduit in the wall and made close made good / surface mounted with required accessories. ","m",200]
[]
[null,"32mm steel Conduit including all necessary accessories. Rate to include chasing wall for conduit in the wall and made close made good / surface mounted with required accessories. ","m",28]
[]
[null,"4-way junction box IP66","No",12]
[]
[null,"100mmX50mm hot deep galvanised draw box recessed mounted on wall ","No",0]
[]
[null,"Supply, deliver to site, store & install P9000 trunking hot dipped galvanised inclusive of all items required to install in accordance with manufacturers specification. Rate must be inclusive of all items such as brackets, raw bolts, splices, bonding straps etc. required to install in accordance with manufacturers specification.","m",300]
[]
[null,"2 compartment PVC powerskirting complete with elbow, internal and external bends, covers and all required accessories. To be grey in colour. ","m",50]
[]
[null,"Supply and install 16A, 3pin, 230V Switched Socket Outlets, white coloured cover plate with red toggle","No",18]
[]
[null,"Supply and install 16A, 2pin/Euro pin, 230V Switched Socket Outlets, red coloured cover plate ","No",21]
[]
[null,"Supply and install 16A, 3pin, earth pin chamfered, 230V Switched Socket Outlets, white coloured cover plate with red toggle","No",15]
[]
[null,"Supply and install 16A, 2pin, 230V Switched Socket Outlets, red coloured cover plate ","No",3]
[]
[null,"LUMINARIES AND CONTROL DEVICES","H2",0]
[]
[null,"Supply, deliver, accept and store the following luminaries, complete with lamps and control gear as per specification. See and refer to the specification document for details of each luminary.","H3",0]
[]
[null,"Type A5 - IP65 Rated, 30W / +/-4440 lm LED - 4000k vapour-proof Surface-mounted weather-proof luminaire, GRP body and acrylic diffuser, with 50000 hours lifespan. ","No",148]
[]
[null,"Type A13 - IP65 Rated, 30W / +/-4440 lm LED - 4000k Rough-guard Surface-mounted weather-proof luminaire, GRP body and acrylic diffuser, with 50000 hours lifespan. ","No",160]
[]
[null,"Type B1 - IP65 Rated high-pressure die cast aluminium base and trim ring 20W/ +/- 2600lm LED - 4000k bulkhead luminaire with an opal high-impact acrylic diffuser, with 50000 hours lifespan. ","No",92]
[]
[null,"Type B3 - IP65 Rated high-pressure die cast aluminium base and trim ring 32W/ +/- 4370lm LED - 4000k bulkhead luminaire with an opal high-impact acrylic diffuser, with 50000 hours lifespan. ","No",44]
[]
[null,"Type B4 - same as B3 above, but with battery backup to operate for 1-hour","No",1]
[]
[null,"Type C4  - 144W / +/-20869lm LED (4000k) Lowbay, rated IP65 with powder coating as per specification","No",52]
[]
[null,"Type C5  -  same as type C4 above, but with battery backup to last 1-hour as per specification","No",0]
[]
[null,"Type C6  - 80W / +/-10000lumen LED (4000k) Floodlight, rated IP65 with powder coating as per specification","No",43]
[]
[null,"Type FL1  - 180W / +/-27000lm LED (4000k) Streetlight rated IP66 with powder coating as per specification","No",53]
[]
[null,"Type FL3  - 54W / +/-7700 lumen LED (4000k) post pole, rated IP65 with powder coating as per specification","No",10]
[]
[null,"Retrofit existing vapour-proof luminiare with LED tube 28W / on a 4ft vapour-proof luminaire. Also removal of electronic balast for a complete operation of the luminiare. ","No",136]
[]
[null,"Photo electric cell as per specification","No",20]
[]
[null,"Supply and installation of 32 Amp 4-Pole surface mounted isolator, complete with all necessary accessories","No",29]
[]
[null,"TEST AND COMMISSIONING ","H2",0]
[]
[null,"CONGELLA STATION ","H3",0]
[]
[null,"Test and commission  the complete electrical installation including completion of quality check sheets, Compliance Certificates & test results and submitting them to the Employer's Representative. ","H3",0]
[]
[null,"Test and commission  the complete electrical installation including Certificates of Compliance & test results to the Engineer.  Main administration ticket office with guard houses.","Item",1,{"v":30000,"d":"30,000.00"},{"v":30000,"d":"R30,000.00"}]
[]
[null,"UMBILO STATION ","H3",0]
[]
[null,"Test and commission  the complete electrical installation including completion of quality check sheets, Compliance Certificates & test results and submitting them to the Employer's Representative. ","H3",0]
[]
[null,"Test and commission  the complete electrical installation including Certificates of Compliance & test results to the Engineer.  ","Item",1,{"v":10000,"d":"10,000.00"},{"v":10000,"d":"R10,000.00"}]
[]
[null,"ROSSBURGH STATION ","H3",0]
[]
[null,"Test and commission  the complete electrical installation including completion of quality check sheets, Compliance Certificates & test results and submitting them to the Employer's Representative. ","H3",0]
[]
[null,"Test and commission  the complete electrical installation including Certificates of Compliance & test results to the Engineer.  ","Item",1,{"v":40000,"d":"40,000.00"},{"v":40000,"d":"R40,000.00"}]
[]
[null,"MEREBANK STATION ","H3",0]
[]
[null,"Test and commission  the complete electrical installation including completion of quality check sheets, Compliance Certificates & test results and submitting them to the Employer's Representative. ","H3",0]
[]
[null,"Test and commission  the complete electrical installation including Certificates of Compliance & test results to the Engineer.  ","Item",1,{"v":35000,"d":"35,000.00"},{"v":35000,"d":"R35,000.00"}]
[]
[null,"BACK-UP GENERATOR","H2",0]
[]
[null,"Congella Station","H3",0]
[]
[null,"Backup diesel Generator - 60kVA, 400VAC three phase, 50Hz, with auto-change over panel. Generator to be installed and supplied with full tank diesel, must be able to Starts & Stops Automatically, Maintenance-free Battery, Silent Weatherproof 3CR12 steel Canopy, Long-range Fuel Tank, Easy Cable Entry, Emergency Stop Button, Weatherproof Exhaust System. ","Item",1,{"v":200000,"d":"200,000.00"},{"v":200000,"d":"R200,000.00"}]
[]
[null,"50 mm² 4c 600/1000V PVC/SWA/PVC ECC Cu Cable ","m",200]
[]
[null,"Cable gland 50 mm² 4c 600/1000V PVC/SWA/PVC ECC Cu Cable","No",2]
[]
[null,"Supporting structure for generator set","Item",1,{"v":80000,"d":"80,000.00"},{"v":80000,"d":"R80,000.00"}]
[]
[null,"Umbilo Station","H3",0]
[]
[null,"Backup diesel Generator - 100kVA, 400VAC three phase, 50Hz, with auto-change over panel. Generator to be installed and supplied with full tank diesel, must be able to Starts & Stops Automatically, Maintenance-free Battery, Silent Weatherproof 3CR12 steel Canopy, Long-range Fuel Tank, Easy Cable Entry, Emergency Stop Button, Weatherproof Exhaust System. ","Item",1,{"v":260000,"d":"260,000.00"},{"v":260000,"d":"R260,000.00"}]
[]
[null,"95 mm² 4c 600/1000V PVC/SWA/PVC ECC Cu Cable ","m",50]
[]
[null,"Cable gland 95mm² 600/1000V PVC/SWA/PVC ECC Cu Cable","No",2]
[]
[null,"Supporting structure for generator set","Item",1,{"v":80000,"d":"80,000.00"},{"v":80000,"d":"R80,000.00"}]
[]
[null,"Rossburgh Station","H3",0]
[]
[null,"Backup diesel Generator - 60kVA, 400VAC three phase, 50Hz, with auto-change over panel. Generator to be installed and supplied with full tank diesel, must be able to Starts & Stops Automatically, Maintenance-free Battery, Silent Weatherproof 3CR12 steel Canopy, Long-range Fuel Tank, Easy Cable Entry, Emergency Stop Button, Weatherproof Exhaust System. ","Item",1,{"v":200000,"d":"200,000.00"},{"v":200000,"d":"R200,000.00"}]
[]
[null,"50 mm² 4c 600/1000V PVC/SWA/PVC ECC Cu Cable ","m",200]
[]
[null,"Cable gland 95mm² 600/1000V PVC/SWA/PVC ECC Cu Cable ","No",2]
[]
[null,"Supporting structure for generator set","Item",1,{"v":80000,"d":"80,000.00"},{"v":80000,"d":"R80,000.00"}]
[]
[null,"Merebank Station","H3",0]
[]
[null,"Backup diesel Generator - 60kVA, 400VAC three phase, 50Hz, with auto-change over panel. Generator to be installed and supplied with full tank diesel, must be able to Starts & Stops Automatically, Maintenance-free Battery, Silent Weatherproof 3CR12 steel Canopy, Long-range Fuel Tank, Easy Cable Entry, Emergency Stop Button, Weatherproof Exhaust System. ","Item",1,{"v":200000,"d":"200,000.00"},{"v":200000,"d":"R200,000.00"}]
[]
[null,"50 mm² 4c 600/1000V PVC/SWA/PVC ECC Cu Cable ","m",100]
[]
[null,"cable gland 50 mm² 4c 600/1000V PVC/SWA/PVC ECC Cu Cable","No",2]
[]
[null,"Supporting structure for generator set","Item",1,{"v":80000,"d":"80,000.00"},{"v":80000,"d":"R80,000.00"}]
[]
[{"$nulls":3},0]
[]
[null,"SECTION NO. 4","H1",0]
[]
[null,"BILL NO. 1 ","H1",0]
[]
[null,"FIRE PROTECTION","H1",0]
[]
[null,"MAIN TICKET OFFICE","H2",0]
[]
[null,"Supply, deliver and install all Fire appliances and  piping with complete with all auxiliary fittings :.","H3",0]
[]
[null,"Everyway hose reel complete with 30m rubber hose, chromium plated stopcock, shut-off nozzle and wall bracket, bolted to wall.","No",8]
[]
[null,"4.5kg Carbon Dioxide fire extinguisher Mounted on a Wooden Block.","No",33]
[]
[null,"Fire Hydrant in a Cabinet","No",2]
[]
[null,"38mm Layflat Hose With Adjustable Nozzle Housed inside a Cabinet","No",2]
[]
[null,"Photoluminated Directional Signage","SUM",3]
[]
[null,"Photoluminated Fire Signage","SUM",3]
[]
[null,"PLATFORMS","H2",0]
[]
[null,"Black Mild Steel Fittings","H3",0]
[]
[null,"25, 90 Degree Threaded Elbow","No",66]
[]
[null,"25mm steel Union","No",44]
[]
[null,"80, 90 Degree Threaded Elbow","No",39]
[]
[null,"80, Equal Threaded Tee","No",34]
[]
[null,"Black Mild Steel Piping","H3",0]
[]
[null,"25 mm Pipes","m",120]
[]
[null,"80 mm Pipes","m",184]
[]
[null,"Supply, deliver and install all Fire appliances and  piping with complete with all auxiliary fittings :.","H3",0]
[]
[null,"Class 16 HDPE Piping & Fittings","H4",0]
[]
[null,"75mm Pipe laid and including trenches not exceeding 800m deep.","m",700]
[]
[null,"25mm Pipe laid and including trenches not exceeding 800m deep.","m",570]
[]
[null,"75mm-25mm Reducing TEE (Flanged)","No",28]
[]
[null,"75mm Adaptor Flange (for fire hydrants)","No",12]
[]
[null,"25mm Adaptor Flange (for FHR lines)","No",20]
[]
[null,"75mm , 90 Degree Elbow","No",130]
[]
[null,"25mm , 90 Degree Elbow","No",30]
[]
[null,"Everyway hose reel complete with 30m rubber hose, chromium plated stopcock, shut-off nozzle and wall bracket, bolted to wall.","No",20]
[]
[null,"4.5kg Carbon Dioxide fire extinguisher Mounted on a Wooden Block.","No",54]
[]
[null,"Fire Hose reel & fire Extinguisher Cabinet","No",20]
[]
[null,"Fire Hydrant in a Cabinet","No",10]
[]
[null,"38mm Layflat Hose With Adjustable Nozzle Housed inside a Cabinet","No",10]
[]
[null,"Photoluminated Directional Signage","SUM",7]
[]
[null,"Photoluminated Fire Signage","SUM",7]
[]
[null,"Fire Brigade Twin Booster Connection","No",4]
[]
[{"$nulls":3},0]
[]
[null,"SECTION NO. 5","H1",0]
[]
[null,"BILL NO. 1 ","H1",0]
[]
[null,"HVAC INSTALLATION","H1",0]
[]
[null,"MAIN TICKET OFFICE","H2",0]
[]
[null,"Supply, deliver and install the following Units as per specification: ","H3",0]
[]
[null,"16 kW Cooling Concealed Ceiling Indoor  Unit","No",3]
[]
[null,"50 kW Multiple System Type Outdoor Condensing Unit Unit","No",1]
[]
[null,"3.6  kW Cooling Midwall split Indoor  Unit","No",2]
[]
[null,"3.6 kW Inverter Type Outdoor Condensing Unit","No",2]
[]
[null,"4  kW Cooling Midwall split Indoor  Unit","No",2]
[]
[null,"4 kW Inverter Type Outdoor Condensing Unit","No",2]
[]
[null,"5  kW Cooling Midwall split Indoor  Unit","No",7]
[]
[null,"5 kW Inverter Type Outdoor Condensing Unit","No",7]
[]
[null,"14  kW Cooling Underceiling Indoor  Unit","No",1]
[]
[null,"14 kW Inverter Type Outdoor Condensing Unit","No",1]
[]
[null,"Refrigeration Copper Piping With Thermal Insulation and all associated Fittings.","m",95]
[]
[null,"PVC Condensate Drain Piping With Insulation","m",75]
[]
[null,"Wired Controller","No",15]
[]
[null,"Provide Full Service and Relocatte The Exixting Midwall Split Unit and The outdoor Condensing Unit","No",5]
[]
[null,"Service the Existing Ducting , Air Terminals and Fresh Air Supply Systems at Rossburgh Station","Item",1,{"v":30000,"d":"30,000.00"},{"v":30000,"d":"R30,000.00"}]
[]
[null,"Fabricate , Supply and Install locable Sercurity Cages around each Outdoor Condensing Unit","No",16]
[]
[null,"Supply The following Ablution Extraction System with Complete Associated Fittings","H3",0]
[]
[null,"400 dia Spiral ducting With Fittings","m",3]
[]
[null,"350 dia Spiral ducting With Fittings","m",3]
[]
[null,"300 dia Spiral ducting With Fittings","m",3]
[]
[null,"250 dia Spiral ducting With Fittings","m",9]
[]
[null,"200 dia Spiral ducting With Fittings","m",9]
[]
[null,"400 dia - 200 Reducing Tee","No",1]
[]
[null,"350 dia - 200 Reducing Tee","No",1]
[]
[null,"300 dia - 200 Reducing Tee","No",2]
[]
[null,"250 dia - 200 Reducing Tee","No",4]
[]
[null,"200 dia 90 Deg Bends","No",12]
[]
[null,"Silencer STD1.5 Melinex","No",4]
[]
[null,"Axial Flow Fan","No",2]
[]
[null,"200 Dia Air Damper","No",6]
[]
[null,"200 Dia Air Valve ","No",11]
[]
[null,"350x250 Door Grille","No",7]
[]
[{"$nulls":3},0]
[]
[null,"SECTION NO.6","H1",0]
[]
[null,"BILL NO. 1","H1",0]
[]
[null,"RETAINING WALL ","H1",0]
[]
[null,"MEREBANK STATION","H1",0]
[]
[null,"PREAMBLES:","H2",0]
[]
[null,"The tenderer is referred to the relevant clauses in the Model Preambles for Trades (2008 Edition) as issued by the Association of South African Quantity Surveyors before pricing this bill",null,0]
[]
[null,"EXCAVATIONS","H2",0]
[]
[null,"Excavating soft material situated within the following successive depth ranges:","H3",0]
[]
[null,"0m up to 1,5m","m3",50]
[]
[null,"Exceeding 1,5m up to 3m","m3",5]
[]
[null,"Extra over for excavation in hard material irrespective of depth","m3",5]
[]
[null,"Backfill to excavations utilising:","H2",0]
[]
[null,"material from the excavation","m3",5]
[]
[null,"imported material","m3",5]
[]
[null,"soil cement, 3% cement","m3",5]
[]
[null,"Fill within a restricted area","m3",5]
[]
[null,"Overhaul","H3",0]
[]
[null,"Overhaul in excess of 1,0km on excavated material and on material imported for backfill and foundation fill","M3.KM",5]
[]
[null,"CONCRETE, FORMWORK AND REINFORCEMENT ","H1",0]
[]
[null,"FALSEWORK, FORMWORK AND CONCRETE FINISH","H2",0]
[]
[null,"Vertical formwork to provide","H3",0]
[]
[null,"Class F1 surface finish to:","H4",0]
[]
[null,"Sides of bases and rear concealed faces of walls","m2",15]
[]
[null,"Joints between adjacent wall panels","m2",20]
[]
[null,"Class F2 surface finish to:","H4",0]
[]
[null,"Front faces of walls","m2",12]
[]
[null,"Class F3 surface finish to:","H4",0]
[]
[null,"Front faces of walls","m2",12]
[]
[null,"REINFORCED CONCRETE","H2",0]
[]
[null,"15MPa/19mm Concrete:","H3",0]
[]
[null,"Blinding","m3",5]
[]
[null,"25MPa/19mm Concrete:","H3",0]
[]
[null,"Foundations","m3",30]
[]
[null,"30MPa/19mm Concrete:","H3",0]
[]
[null,"Retaining Wall","m3",30]
[]
[null,"SUPERSTRUCTURE","H2",0]
[]
[null,"Brickwork of NFX bricks (14 MPa nominal compressivestrength) in class II mortar in load bearing walls etc","H3",0]
[]
[null,"Piers","m3",1]
[]
[null,"H-shaped Piers","m3",1]
[]
[null,"Half brick walls","m2",1]
[]
[null,"One brick walls","m2",1]
[]
[null,"280mm hollow walls of two half brick skins including wire ties","m2",1]
[]
[null,"One and a half brick wall","m2",100]
[]
[null,"390mm hollow walls of one half brick and one one brick skins including wire ties","m2",1]
[]
[null,"Two brick walls","m2",1]
[]
[null,"BRICKWORK SUNDRIES","H2",0]
[]
[null,"Brickwork reinforcement:","H3",0]
[]
[null,"75mm Wide reinforcement built in horizontally","m",1]
[]
[null,"150mm Wide reinforcement built in horizontally","m",1]
[]
[null,"230mm Wide reinforcement built in horizontally","m",200]
[]
[]
[null,"PRELIMINARIES"]
[]
[null,"BUILDER'S WORK"]
[]
[null,"ELECTRICAL INSTALLATION"]
[]
[null,"FIRE PROTECTION"]
[]
[null,"HEATING, VENTILATION AND AIR-CONDITIONING"]
[]
[null,"EXTERNAL WORKS"]
[]
[null,"SUB-TOTAL","ST"]
[]
[null,"ADD 10% CONTINGENCIES TO BE USED AT THE CLIENT AND PRINCIPAL AGENTS DISCRETION","TAX",{"v":0.1,"d":"10%"}]
[]
[null,"SUB-TOTAL","ST"]
[]
[null,"ADD VAT","TAX",{"v":0.15,"d":"15%"}]
[]
[null,"TOTAL","T"]