{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":7,"n_cols":6,"rows_kept":7}
["Item","Material","Description","Quantity","Rate","Price"]
[1,"Sap: 0010309","BUSHING: TYPE: RIP/RIS; VOLTAGE: 123 KV; CURRENT: 1.25 KA; BASIC INSULATION LEVEL: 550 KV; CURRENT TRANSFORMER EXTENSION DIAMETER: 140 MM; CURRENT TRANSFORMER EXTENSION: 300 MM; OIL EXTENSION: 560 MM; FLANGE DIAMETER: 290 MM; MOUNTING HOLES: 8 X 16 MM; PITCH CIRCLE DIAMETER: 250 MM; STEM DIAMETER: 38 MM",null,null,{"$f":"E2*D2","v":0}]
[2,"Sap: 0010640","BUSHING: TYPE: RIP/RIS; VOLTAGE: 132 KV; CURRENT: 1.25 KA; BASIC INSULATION LEVEL: 650 KV; CURRENT TRANSFORMER EXTENSION DIAMETER: 160 MM; CURRENT TRANSFORMER EXTENSION: 300 MM; OIL EXTENSION: 660 MM; FLANGE DIAMETER: 290 MM; MOUNTING HOLES: 8 X 16 MM; PITCH CIRCLE DIAMETER: 250 MM; STEM DIAMETER: 38; LIGHTNING IMPULSE; 550 KV; SWITCHING IMPULSE: 470 KV; FLANGE EXTENSION: 300 MM; LENGTH OIL SIDE: 680 MM;BASE FLANGE: 335 DIAMETER; FLANGE EXTENSION: 160 DIAMETER; MOUNTING HOLES: 12 X 16 DIAMETER; PCD 290; LINE TERMINAL 38 DIAMETER; LINE TERMINAL LENGTH: 125",null,null,{"$f":"E3*D3","v":0}]
[3,"Sap: 0402466","BUSHING: TYPE: RIP/RIS; VOLTAGE: 52 KV; CURRENT: 1000 A; BASIC INSULATION LEVEL: 250 KV; CURRENT TRANSFORMER EXTENSION DIAMETER: 130 KV; CURRENT TRANSFORMER EXTENSION: 300 MM; OIL EXTENSION: 440 MM; FLANGE DIAMETER: 290 MM; MOUNTING HOLES: 8 X 16 MM; PITCH CIRCLE DIAMETER: 250 MM; STEM DIAMETER: 26 MM",null,null,0]
[4,"Sap: 0402474","BUSHING: TYPE: RIP/RIS; VOLTAGE: 52 KV; CURRENT: 2.5 KA; BASIC INSULATION LEVEL: 250 KV; CURRENT TRANSFORMER EXTENSION DIAMETER: 130 MM; CURRENT TRANSFORMER EXTENSION: 300 MM; OIL EXTENSION: 440 MM; FLANGE DIAMETER: 290 MM; MOUNTING HOLES: 8 X 16 MM; PITCH CIRCLE DIAMETER: 250 MM; STEM DIAMETER: 38 MM",null,null,0]
[]
[{"$nulls":5},{"$f":"SUM(F2:F5)","v":0}]