{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"defined_names":2},"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":107,"n_cols":3,"rows_kept":107,"merged":[[20,0,20,2],[30,0,30,2],[33,0,33,2],[38,0,38,2],[41,0,41,2],[47,0,47,2],[59,0,59,2],[71,0,71,2],[83,0,83,2]]}
["Item","Description","QTY"]
[null,"Limpopo LSAC: Schoemansdal Museum"]
[null,"1. Sever room / Clean MAT"]
[1,"UTP CAT6 Data Point complete with 3m flylead and patchlead",2]
[2,"ADAPTER 22.5 X 45 LEGRAND HK SHUTTER",2]
[{"$f":"A5+1","v":3},"KEYSTONE RJ45 KM8 C6 WHITE STP",2]
[4,"Cover Plate P/O 50x50 E/O",2]
[5,"Collar 50x50",2]
[6,"Euromod Half Blank White",2]
[7,"Electrical Normal Power Point  complete, excl CB.",5]
[8,"Electrical Dedicated Power Point  complete, excl CB.",5]
[9,"Cover 2 X 4 Vert White 16 Amp",5]
[10,"Cover Socket 2 X 4 Vert Red Ded 16 Amp For MS2",5]
[11,"Plugtop 16 Amp Red",5]
[12,"Switch 48 PORT POE",1]
[13,"BRADY \"0\" - \"9\" 37/STRIP BLACK/WHITE",2]
[14,"BRUSH PANEL SHORT BASE METAL",4]
[15,"24 PORT PATCH PANEL CAT 6e LOADED",2]
[16,"25U Cabinet. (Includes UPS, power surge protection, cabinet management, etc.)",1]
[17,"Smart-UPS, 900 Watts /1500 VA, Input 230V /Output 230V, Interface Port USB, Floor Standing",1]
["2. WORK ROOM"]
[1,"UTP CAT6 Data Point complete with 3m flylead and patchlead",6]
[{"$f":"A22+1","v":2},"ADAPTER 22.5 X 45 LEGRAND HK SHUTTER",6]
[{"$f":"A23+1","v":3},"KEYSTONE RJ45 KM8 C6 WHITE STP",6]
[{"$f":"A24+1","v":4},"Cover Plate P/O 50x50 E/O",6]
[{"$f":"A25+1","v":5},"Collar 50x50",6]
[{"$f":"A26+1","v":6},"Euromod Half Blank White",6]
[7,"Electrical Normal Power Point  complete, excl CB.",2]
[8,"Cover 2 X 4 Vert White 16 Amp",2]
[9,"Cable Surfex 2.5 X 2 Core + Earth Dedicated plugs & normal plugs","120m"]
["3. STAFF ROOM"]
[1,"Acess point for WIFI AP, Surface mount CAT 6 Wall box, installed just outside room on ceiling",2]
[2,"Internal Ceiling mount access point",1]
["4. RECEPTION"]
[1,"Access point for WIFI AP, Surface mount CAT 6 Wall box",2]
[2,"Access point for WIFI AP, Surface mount CAT 6 Wall box, 2x@ entrance &2@ opposite",4]
[3,"external / outside wall mounted access point",2]
[4,"Internal Ceiling mount access point",1]
["5. BOARD ROOM"]
[1,"Access point for WIFI AP, Surface mount CAT 6 Wall box",2]
[{"$f":"A40+1","v":2},"Internal Ceiling mount access point",1]
["6. OFFICE: FOREMAN"]
[1," UTP CAT6 Data Point complete with 3m flylead and patchlead",2]
[{"$f":"A43+1","v":2},"ADAPTER 22.5 X 45 LEGRAND HK SHUTTER",2]
[{"$f":"A44+1","v":3},"KEYSTONE RJ45 KM8 C6 WHITE STP",2]
[{"$f":"A45+1","v":4},"Cover Plate P/O 50x50 E/O",2]
[{"$f":"A46+1","v":5},"Collar 50x50",2]
["7. OFFICE 1"]
[1," UTP CAT6 Data Point complete with 3m flylead and patchlead",2]
[{"$f":"A49+1","v":2},"ADAPTER 22.5 X 45 LEGRAND HK SHUTTER",2]
[{"$f":"A50+1","v":3},"KEYSTONE RJ45 KM8 C6 WHITE STP",2]
[{"$f":"A51+1","v":4},"Cover Plate P/O 50x50 E/O",2]
[{"$f":"A52+1","v":5},"Collar 50x50",2]
[6,"Electrical Normal Power Point  complete, excl CB.",1]
[7,"Electrical Dedicated Power Point  complete, excl CB.",1]
[8,"Cover 2 X 4 Vert White 16 Amp",1]
[9,"Cover Socket 2 X 4 Vert Red Ded 16 Amp For MS2",1]
[10,"Plugtop 16 Amp Red",1]
[11,"Cable Surfex 2.5 X 2 Core + Earth Dedicated plugs & normal plugs","40M"]
["8. OFFICE 2"]
[1," UTP CAT6 Data Point complete with 3m flylead and patchlead",4]
[{"$f":"A61+1","v":2},"ADAPTER 22.5 X 45 LEGRAND HK SHUTTER",4]
[{"$f":"A62+1","v":3},"KEYSTONE RJ45 KM8 C6 WHITE STP",4]
[{"$f":"A63+1","v":4},"Cover Plate P/O 50x50 E/O",4]
[{"$f":"A64+1","v":5},"Collar 50x50",4]
[6,"Electrical Normal Power Point  complete, excl CB.",1]
[7,"Electrical Dedicated Power Point  complete, excl CB.",1]
[8,"Cover 2 X 4 Vert White 16 Amp",1]
[9,"Cover Socket 2 X 4 Vert Red Ded 16 Amp For MS2",1]
[10,"Plugtop 16 Amp Red",1]
[11,"Cable Surfex 2.5 X 2 Core + Earth Dedicated plugs & normal plugs","50M"]
["9. OFFICE 3"]
[1," UTP CAT6 Data Point complete with 3m flylead and patchlead",4]
[{"$f":"A73+1","v":2},"ADAPTER 22.5 X 45 LEGRAND HK SHUTTER",4]
[{"$f":"A74+1","v":3},"KEYSTONE RJ45 KM8 C6 WHITE STP",4]
[{"$f":"A75+1","v":4},"Cover Plate P/O 50x50 E/O",4]
[{"$f":"A76+1","v":5},"Collar 50x50",4]
[6,"Electrical Normal Power Point  complete, excl CB.",1]
[7,"Electrical Dedicated Power Point  complete, excl CB.",1]
[8,"Cover 2 X 4 Vert White 16 Amp",1]
[9,"Cover Socket 2 X 4 Vert Red Ded 16 Amp For MS2",1]
[10,"Plugtop 16 Amp Red",1]
[11,"Cable Surfex 2.5 X 2 Core + Earth Dedicated plugs & normal plugs","60M"]
["10. OFFICE 4"]
[1," UTP CAT6 Data Point complete with 3m flylead and patchlead",4]
[{"$f":"A85+1","v":2},"ADAPTER 22.5 X 45 LEGRAND HK SHUTTER",4]
[{"$f":"A86+1","v":3},"KEYSTONE RJ45 KM8 C6 WHITE STP",4]
[{"$f":"A87+1","v":4},"Cover Plate P/O 50x50 E/O",4]
[{"$f":"A88+1","v":5},"Collar 50x50",4]
[6,"Electrical Normal Power Point  complete, excl CB.",1]
[7,"Electrical Dedicated Power Point  complete, excl CB.",1]
[8,"Cover 2 X 4 Vert White 16 Amp",1]
[9,"Cover Socket 2 X 4 Vert Red Ded 16 Amp For MS2",1]
[10,"Plugtop 16 Amp Red",1]
[11,"Cable Surfex 2.5 X 2 Core + Earth Dedicated plugs & normal plugs","65M"]
[null,"Documentation"]
[{"$f":"A96+1","v":1},"Test Data Point",34]
[2,"UTP Labelling",68]
[3,"Power Labelling",10]
[4,"Schematic Layout Of Network",3]
[5,"Data Certification",1]
[6,"UTP Test Results",1]
[7,"COC - Electrical Certification",1]
[null,"SUNDRIES/ Infrasrtucture"]
[{"$f":"A104+1","v":1},"Tape Brother White 9mm / BRADY \"0\" - \"9\" 37/STRIP BLACK/WHITE",2]
[2,"Insulation Tape - Black",2]
[3,"25a, Circuit Breaker, Std Curve",1]