{"text_format":"3","workbook":"xls","n_sheets":11,"sheets":["Cover Page ","1.) Scope of Work","2.) BoQ Summary","Preliminaries","Compliance","1.) Tanks, pumps, etc.","2.) Fans","Basement - 2","Basement - 1","Ground Floor ","First Floor "],"not_rendered":{"images":1,"external_links":1,"defined_names":5},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Cover Page ","index":0,"n_rows":47,"n_cols":5,"rows_kept":47,"merged":[[42,0,42,1],[43,0,43,1],[45,1,45,2],[46,1,46,2],[47,1,47,2],[48,1,48,2],[49,1,49,2]],"flags":["formulas_cached_only"]}
{"$rows_empty":30}
["PROJECT: ",null,"1.) Water Tanks and pumps for Secunda (2 off)"]
[null,null,"2.) Fans for Secunda (7 off)"]
[]
[]
[]
["DOCUMENT NAME: ",null,"SoW AND  BoQ"]
[]
[]
[]
["The following signatories have approved the report:"]
[]
["Name",null,"Purpose"]
["Cornelis van Hoeve",null,"Generated"]
["Fannie Raseruthe",null,"Checked"]
[]
["Rev","Description",null,"Author","Pages"]
["A","Issued for Tender",null,"CvH","All"]

{"sheet":"1.) Scope of Work","index":1,"n_rows":38,"n_cols":6,"rows_kept":38,"flags":["formulas_cached_only"]}
[]
["No","Description","Unit","Qty","Rate","Amount"]
[null," "]
[]
[null,"Scope of Work : 2 x Emergency Water tanks"]
[]
[null,"This BOQ is to be read inconjuction with the Scope of Work "]
[]
[null,"Where trades names are used, it shall be read to include the phrase \"or approved equal\"."]
[]
[null,"\"Rate\" includes material, mark-up & installation labour."]
[]
[null,"All breaking and making good of building & paving due to equipment penetrations shall be allowed for "]
[]
[null,"All items on the Bill are re-measurable"]
[]
[null,"1.) Water Tanks with pumps etc to server as backup water ( 2 off)\nThe work requires the installation of 2 x Jojo Tanks (5000 L) at the 2 premises occupied by SABS in Secunda, i.e. 5 & 8 Bunsen street."]
[]
[null,"See attached drawing for a proposal. The supplier can impprove on this design if so required."]
[]
[null,"2.) Fans for oven room extraction (2 off)"]
[null,"Supply and install Fans (2 off)"]
[null,"min flow - 3500 m3/h"]
[null,"Min pressure 120Pa"]
[]
[null,"Fans to be insatlled at 2nd floor level inside existing blue boxes."]
[null,"Sizesof blue box approxamately 500 x 500 mm (to be confirmed by contractor)."]
[null,"Estimated max fan diameter 400 mm -TBC by contractor."]
[null,"Electrical connection according to requirements"]
[null,"CoC for insatllation"]
[]
[]
[null,"3.) Fans for chemical starage room extraction (5 off)"]
[null,"Supply and install Fans  (Light commercial)"]
[null,"min flow - 800 m3/h"]
[null,"Min pressure 70Pa"]
[null,"Electrical connection according to requirements"]
[null,"CoC for insatllation"]

{"sheet":"2.) BoQ Summary","index":2,"n_rows":25,"n_cols":6,"rows_kept":25,"flags":["formulas_cached_only"]}
["No","Description",{"$nulls":3},"Amount"]
[]
[null,"Secunda 2 x water tanks with pumps, etc"]
[]
["A","SUMMARY"]
[]
["B","Preliminary and General",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
["C","Compliance",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[]
["D","Tanks, pumps, fittings, pipes, etc.",{"$nulls":3},{"v":30000,"d":"R 30,000.00"}]
[]
["E","Fans and Installation",{"$nulls":3},{"v":30000,"d":"R 30,000.00"}]
{"$rows_empty":7}
[null,"TOTAL",{"$nulls":3},{"v":60000,"d":"R 60,000.00"}]
[]
[null,"ADD VAT (15%)",{"$nulls":3},{"v":9000,"d":"R 9,000.00"}]
[]
[null,"GRAND TOTAL",{"$nulls":3},{"v":69000,"d":"R 69,000.00"}]

{"sheet":"Preliminaries","index":3,"n_rows":40,"n_cols":6,"rows_kept":40,"flags":["formulas_cached_only"]}
[]
["No","Description",null,"Qty","Rate","Amount"]
[null," "]
["B","PRELIMINARY AND GENERAL"]
[]
[null,"Note: All items shall be priced for whatever cost may be consider necessary for Preliminary and General to carry out the Mechanical Installations in full, as detailed in the drawings, Specifications and Schedules, which shall include, but shall not be limited, to the following:"]
[]
["B1","Site establishment-over and above the main contractors including the removal thereof upon completion","Item",1,null,{"v":0,"d":"R 0.00"}]
[]
["B2","Company Head Office overhead costs","Item",1,null,{"v":0,"d":"R 0.00"}]
[]
["B3","Workshop drawings and equipment submittals","Item",1,null,{"v":0,"d":"R 0.00"}]
[]
["B4","Project engineering and management including coordination with other services on site","Item",1,null,{"v":0,"d":"R 0.00"}]
[]
["B5","Instructing and training the Employer's staff in operation of system and equipment prior to hand over to the Client.","Item",1,null,{"v":0,"d":"R 0.00"}]
[null," "]
["B6","Three copies of the O&M Manuals (hard copies and USB)","Item",1,null,{"v":0,"d":"R 0.00"}]
[]
["B7","As-Built Drawings (3 copies)","Item",1,null,{"v":0,"d":"R 0.00"}]
[null," "]
["B8","Any necessary calculations requested by the Engineer.","Item",1,null,{"v":0,"d":"R 0.00"}]
[]
["B9","12 month guarantee period","Item",1,null,{"v":0,"d":"R 0.00"}]
[]
["B10","Provision of full maintenance and guarantee of mechanical equipment and installation for the full 12 month period. The maintenance period shall start after practical completion is achieved.  Service sheets to be submitted for every service carried out.  ","Item",1,null,{"v":0,"d":"R 0.00"}]
{"$rows_empty":13}
[null,"SUBTOTAL CARRIED FORWARD TO SUMMARY",{"$nulls":3},{"v":0,"d":"R 0.00"}]

{"sheet":"Compliance","index":4,"n_rows":27,"n_cols":6,"rows_kept":27,"flags":["formulas_cached_only"]}
[]
["No","Description",null,"Qty","Rate","Amount"]
[null," "]
["C","COMPLIANCE"]
[]
[null,"Note: All items shall be priced for whatever cost may be consider necessary for Compliance to carry out the Mechanical Installations in full, as detailed in the drawings, Specifications and Schedules, which shall include, but shall not be limited, to the following:"]
[]
["C1","Compliance with OHS Regulations (latest version) and Site Specific Health & Safety Specification","Item",1,null,{"v":0,"d":"R 0.00"}]
[]
["C2","Clearing of rubble and housekeeping","Item",1,null,{"v":0,"d":"R 0.00"}]
[]
["C3","Scaffolding (3 m high)","Item",1,null,{"v":0,"d":"R 0.00"}]
[]
["C4","Protection of Equipment against damage during construction","Item",1,null,{"v":0,"d":"R 0.00"}]
[]
["C5","Transport and delivery","Item",1,null,{"v":0,"d":"R 0.00"}]
[]
["C6","Rigging and crane hire (2 TANKS)","Item",1,null,{"v":0,"d":"R 0.00"}]
[]
["C7","Provision of spare parts and all related accessories as per specification","Item",1,null,{"v":0,"d":"R 0.00"}]
[]
["C8","Workshop drawings","Item",1,null,{"v":0,"d":"R 0.00"}]
[]
["C9","Testing, commissioning and handing over in full working order of entire system(s).","Item",1,null,{"v":0,"d":"R 0.00"}]
[]
[]
[null,"SUBTOTAL CARRIED FORWARD TO SUMMARY",{"$nulls":3},{"v":0,"d":"R 0.00"}]

{"sheet":"1.) Tanks, pumps, etc.","index":5,"n_rows":43,"n_cols":6,"rows_kept":43,"flags":["formulas_cached_only"]}
["No","Description",null,"Qty","Rate","Amount"]
[]
[]
[]
[]
["D1","2 x Tanks with pumps, pipes, non return valves, ball valves, piping, all fittings, electrical supply, cabling, breakers, isolators and all other equipment to complete this project."]
[]
[]
[]
["D1.2","5000 L JoJo tanks","Qty",2,null,{"v":0,"d":"R 0.00"}]
[]
["D1.3","Pressure pump with build in adjustable pressure switch","Qty",2,null,{"v":0,"d":"R 0.00"}]
[null,"Single phase 230 V"]
[null,"Min flow rate : 3000 L/h"]
[]
["D1.4","Non return valves 1.5 \"","Qty",6,null,{"v":0,"d":"R 0.00"}]
[]
["D1.5","50 mm Class 16 HDPE pipe","Qty",200,null,{"v":0,"d":"R 0.00"}]
[]
["D1.6","T- Pieces (External compression fittings) 50 mm","Qty",10,null,{"v":0,"d":"R 0.00"}]
[]
["D1.7","Elbows- (External compression fittings) 50 mm","Qty",10,null,{"v":0,"d":"R 0.00"}]
[]
["D1.8","50 mm BSP to 50 mm External compression fittings adapters","Qty",10,null,{"v":0,"d":"R 0.00"}]
[]
["D1.9","JoJo tank to 50 mm External compression fittings adapters","Qty",6,null,{"v":0,"d":"R 0.00"}]
[]
["D1.10","Ball valve assembly for JoJo tank top","Qty",3,null,{"v":0,"d":"R 0.00"}]
[]
["D1.11","SurFix electrical cable (2 + earth) 2.5 mm2","m",100,null,{"v":0,"d":"R 0.00"}]
[]
["D1.12","Isolator ","Qty",2,null,{"v":0,"d":"R 0.00"}]
[]
["D1.13","Breaker (10 A) installed in DB","Qty",3,null,{"v":0,"d":"R 0.00"}]
[]
["D1.14","Trenching","m2",10,null,{"v":0,"d":"R 0.00"}]
[]
["D1.15","Re- establish paving","m2",100,null,{"v":0,"d":"R 0.00"}]
[]
["D1.16","Contingency","Amount",1,{"v":30000,"d":"R 30,000.00"},{"v":30000,"d":"R 30,000.00"}]
[]
[]
[null,"SUBTOTAL CARRIED FORWARD TO SUMMARY",{"$nulls":3},{"v":30000,"d":"R 30,000.00"}]

{"sheet":"2.) Fans","index":6,"n_rows":37,"n_cols":6,"rows_kept":37,"flags":["formulas_cached_only"]}
["No","Description",null,"Qty","Rate","Amount"]
[]
[]
[]
[]
["D1","2 x Fans with all caballing and installation"]
[]
["E1.1","Supply and install Fans (2 off)"]
[null,"min flow - 3500 m3/h"]
["E1.2","Min pressure 120Pa","Rate",2,null,{"v":0,"d":"R 0.00"}]
[null,"Duty cycle 24h per day, 365 days per year i.e. 24 h continuous"]
[]
["E1.3","SurFix electrical cable (2 + earth) 2.5 mm2","m",100,null,{"v":0,"d":"R 0.00"}]
[]
["E1.4","Isolator ","Rate",2,null,{"v":0,"d":"R 0.00"}]
[]
["E1.5","Breaker (10 A) installed in DB","Rate",2,null,{"v":0,"d":"R 0.00"}]
[]
["E1.6","CoC certificate issued","Rate",1,null,{"v":0,"d":"R 0.00"}]
[]
["E1.7","Access to 2 nd floor for installation (Scaffold, ladders, etc)","Amount",1,null,{"v":0,"d":"R 0.00"}]
[]
["E1.8","Labour for installation for 2 fans, electrical supply and all other requirements","Amount",2,null,{"v":0,"d":"R 0.00"}]
[]
["E1.9","Supply door grill (1 x 1 m) and install","Amount",1,null,{"v":0,"d":"R 0.00"}]
[]
[null,"Supply and instal Fans for chemical starage room extraction (5 off)"]
[null,"Supply and install Fans  (Light commercial)","Rate",5,null,{"v":0,"d":"R 0.00"}]
[null,"min flow - 800 m3/h"]
[null,"Min pressure 70Pa"]
[null,"Electrical connection according to requirements"]
[null,"CoC for insatllation"]
[]
["E1.9","Contingency","Amount",1,{"v":30000,"d":"R 30,000.00"},{"v":30000,"d":"R 30,000.00"}]
[]
[]
[null,"SUBTOTAL CARRIED FORWARD TO SUMMARY",{"$nulls":3},{"v":30000,"d":"R 30,000.00"}]

{"sheet":"Basement - 2","index":7,"n_rows":115,"n_cols":6,"rows_kept":115,"hidden":true,"flags":["formulas_cached_only"]}
["No","Description","Unit","Qty","Rate","Amount"]
["G","HVAC - Basement - 2"]
[]
[null,"Air-Conditioning "]
[]
["G1","DX type Inverter Split Unit (Guard House)"]
[]
[null,"Supply, deliver and install a mid-wall split air conditioning unit complete with indoor and outdoor unit. Including decorative panel, piping between indoor and outdoor portion of unit, mounting brackets, condensate drain pumps and all necessary accessories."]
[]
["G1.2","Brand: Midea, LG, Daikin, Samsung or similar approved ","No",1]
[null,"Type: Midwall, Cassette, Hide-away, Under-ceiling"]
[null,"Cooling Capacity: (BTU or KW)"]
[null,"Heating capacity: (BTU or KW)"]
[null,"Reverse Cycle, cooling only, heating only "]
[null,"Refrigerant: "]
[null,"Inverter Type, Non-Inverter type "]
[null,"Controller: Wired or Wireless"]
[]
["G1.2","Supply and install wired wall mounted remote controller with temperature display, temperature set point, 3 fan speeds, heat/cool mode and ON/OFF functions.","No",1]
[]
["G1.3","Apply anti-corrosion treatment on all the condenser coils (Bluchem or equally approved). Certificate of treatment to be submitted to the design engineer. (Rate per split unit)","No",1]
[]
["G1.4","Additional Piping between Indoor and Outdoor unit including pipe ancillaries, wire mesh tray, pipe supports and installation ancillaries","m",1]
[]
["G2","Extraction System "]
[]
[null,"Supply, deliver and install the following items:"]
[]
["G2.1","Extract Fan (Waste Area)","No",1]
[null,"Fan Type: In-line Axial Fan, Centrifugal Fan, Wall Mounted "]
[null,"Fan Make: ………...or equal and approved"]
[null,"Fan Size: …….diameter or ….x….."]
[null,"Process Data: Airflow (L/s) @ Pressure"]
[null,"Rotational Speed: ……….rpm"]
[null,"Mounting: Anti-Vibration Mounts, Ceiling/Wall mounting kit "]
[null,"Motor Size: (KW)"]
[]
["G2.2","Sound Attenuator","No",2]
[null,"Diameter to suit fan, with flexible collars"]
[null,"Length: 600L, 900L"]
[null,"POD type"]
[null,"NC rating: 35"]
[]
["G2.3","Weather Louver","No",1]
[null,"Make: ………...or equal and approved"]
[null,"Model:  ………...or equal and approved"]
[null,"Size: "]
[null,"Finish: Epoxy Powder Coated or Aluminium Anodised"]
[null,"Hinged with Washable pleated Filter"]
{"$rows_empty":7}
[null,"TOTAL CARRIED FORWARD"]
[]
["No","Description","Unit","Qty","Rate","Amount"]
[null," "]
[null,"TOTAL BROUGHT DOWN"]
[]
["G2.4","Extract Air Grille","No",1]
[null,"Make: "]
[null,"Type: Egg Crate, disc valve"]
[null,"Size: "]
[null,"Finish: Epoxy Powder Coated, Aluminium Anodised or Standard colour to Arch's specification."]
[null,"Opposed Blade Damper (OBD): Y/N"]
[]
["G2.5","Door Grille","No",1]
[null,"Make: "]
[null,"Size: "]
[null,"Finish: Epoxy Powder Coated, Aluminium Anodised or Standard colour to Arch's specification."]
[]
["G2.6","Control Box for fan to switch on when lights are operational, position can be in service shaft, weather proof box with cabling and ancillaries or 24/7 timer","No",1]
[]
["G2.7","Ducting"]
[null,"Low Pressure Galvanised ducting including flexible connections, transformation pieces, bends, shoe pieces, spogots, stop ends and all duct fittings to SANS 1238, \"S\" slip & Drive Slip, 0.6mm ","Sqm"]
[null,"Category 1"]
[]
["G2.8","Flexible Duct"]
[null,"Supply and install wire reinforced aluminium flexible ducting complete with clamps; duct sealant and fixings. 1 500 long","No",1]
[null,"Diameter: "]
[]
["G2.9","Balancing Damper "]
[null,"Balancing Damper to suit duct, manual type, made of sheet metal","No",1]
[null,"Size: "]
[]
["G2.10","Fire Damper "]
[null,"2 hour fire rated Fire Damper with Fusible Link or motorised ","No",1]
[null,"Size: "]
[]
["G2.11","Extract Fan (Guard house toilet)","No",1]
[null,"Fan Type: Ceiling Mounted "]
[null,"Fan Make: ………...or equal and approved"]
[null,"Fan Size: …….diameter or ….x….."]
[null,"Process Data: Airflow (L/s) @ Pressure"]
[null,"Rotational Speed: ……….rpm"]
[null,"Mounting: Anti-Vibration Mounts, Ceiling/Wall mounting kit "]
[null,"Motor Size: (KW)"]
[]
["G2.12","Door Grille","No",1]
[null,"Make: "]
[null,"Size: "]
[null,"Finish: Epoxy Powder Coated, Aluminium Anodised or Standard colour to Arch's specification."]
[]
["G2.13","Control Box for fan to switch on when lights are operational","No",1]
{"$rows_empty":7}
[null,"SUBTOTAL CARRIED FORWARD TO SUMMARY"]

{"sheet":"Basement - 1","index":8,"n_rows":166,"n_cols":6,"rows_kept":166,"hidden":true,"flags":["formulas_cached_only"]}
["No","Description",null,"Qty","Rate","Amount"]
["H","HVAC - Basement - 1"]
[]
[null,"Air-Conditioning "]
[]
["H1","DX type Inverter Split Unit"]
[]
[null,"Supply, deliver and install a DX type inverter split unit complete with indoor and outdoor unit including piping between indoor and outdoor portion of unit, mounting brackets, condensate drain pumps and all necessary accessories."]
[]
["H1.2","Brand: Midea, LG, Daikin, Samsung or similar approved ","No",1]
[null,"Type: Hide-away (DV Retail Area)"]
[null,"Cooling Capacity: (BTU or KW)"]
[null,"Heating capacity: (BTU or KW)"]
[null,"Reverse Cycle, cooling only, heating only "]
[null,"Refrigerant: "]
[null,"Inverter Type, Non-Inverter type "]
[null,"Controller: Wired or Wireless"]
[]
["H1.3","Brand: Midea, LG, Daikin, Samsung or similar approved ","No",1]
[null,"Type: Cassette c/w decorative panel (BOH/Receiving/Office)"]
[null,"Cooling Capacity: (BTU or KW)"]
[null,"Heating capacity: (BTU or KW)"]
[null,"Reverse Cycle, cooling only, heating only "]
[null,"Refrigerant: "]
[null,"Inverter Type, Non-Inverter type "]
[null,"Controller: Wired or Wireless"]
[]
["H1.4","Supply and install wired wall mounted remote controller with temperature display, temperature set point, 3 fan speeds, heat/cool mode and ON/OFF functions.","No",2]
[]
["H1.5","Apply anti-corrosion treatment on all the condenser coils (Bluchem or equally approved). Certificate of treatment to be submitted to the design engineer. (Rate per split unit)","No",2]
[]
["H1.6","Additional Piping between Indoor and Outdoor unit including pipe ancillaries, wire mesh tray, pipe supports and installation ancillaries","m",1]
[]
["H2","Basement Parking Ventilation System"]
[]
[null,"Supply, deliver and install the following items:"]
[]
["H2.1","Ventilation Fan ","No",1]
[null,"Fan Type: In-line Axial Fan, Centrifugal Fan, Wall Mounted "]
[null,"Fan Make: ………...or equal and approved"]
[null,"Fan Size: …….diameter or ….x….."]
[null,"Process Data: Airflow (L/s) @ Pressure"]
[null,"Rotational Speed: ……….rpm"]
[null,"Mounting: Anti-Vibration Mounts, Ceiling/Wall mounting kit "]
[null,"Motor Size: (KW)"]
[]
["H2.2","Sound Attenuator","No",2]
[null,"Diameter to suit fan, with flexible collars"]
[null,"Length: 600L, 900L"]
[null,"POD type"]
[null,"NC rating: 35"]
[]
[]
[]
[]
[]
[]
[null,"TOTAL CARRIED FORWARD"]
[]
["No","Description","Unit","Qty","Rate","Amount"]
[null," "]
[null,"TOTAL BROUGHT DOWN"]
[]
["H2.3","Weather Louver","No",1]
[null,"Make: ………...or equal and approved"]
[null,"Model:  ………...or equal and approved"]
[null,"Size: "]
[null,"Finish: Epoxy Powder Coated or Aluminium Anodised"]
[null,"Hinged with Washable pleated Filter"]
[]
["H2.4","Control Box for fan to switch on when lights are operational, position can be in service shaft, weather proof box with cabling and ancillaries or 24/7 timer","No",1]
[]
["H2.5","Ducting"]
[null,"Low Pressure Galvanised ducting including all transformation pieces (including all brackets and supports) to SANS 1238, \"S\" slip & Drive Slip, 0,6mm ","Sqm"]
[null,"Category 1"]
[]
["H2.6","Inlet Cone"]
[null,"Supply and install fan inlet cone complete with bird proof wire mesh screen.","No",1]
[null,"Size: "]
[]
["H3","Alignment & Fitment Ventilation System"]
[]
[null,"Supply, deliver and install the following items:"]
[]
["H3.1","Ventilation Fan ","No",1]
[null,"Fan Type: In-line Axial Fan, Centrifugal Fan, Wall Mounted "]
[null,"Fan Make: ………...or equal and approved"]
[null,"Fan Size: …….diameter or ….x….."]
[null,"Process Data: Airflow (L/s) @ Pressure"]
[null,"Rotational Speed: ……….rpm"]
[null,"Mounting: Anti-Vibration Mounts, Ceiling/Wall mounting kit "]
[null,"Motor Size: (KW)"]
[]
["H3.2","Sound Attenuator","No",2]
[null,"Diameter to suit fan, with flexible collars"]
[null,"Length: 600L, 900L"]
[null,"POD type"]
[null,"NC rating: 35"]
[]
["H3.3","Weather Louver","No",1]
[null,"Make: ………...or equal and approved"]
[null,"Model:  ………...or equal and approved"]
[null,"Size: "]
[null,"Finish: Epoxy Powder Coated or Aluminium Anodised"]
[null,"Hinged with Washable pleated Filter"]
[]
["H3.4","Control Box for fan to switch on when lights are operational, position can be in service shaft, weather proof box with cabling and ancillaries or 24/7 timer","No",1]
[]
["H3.5","Ducting"]
[null,"Low Pressure Galvanised ducting including all transformation pieces (including all brackets and supports) to SANS 1238, \"S\" slip & Drive Slip, 0,6mm ","Sqm"]
[null,"Category 1"]
[]
[]
[]
[]
[null,"TOTAL CARRIED FORWARD"]
[]
["No","Description","Unit","Qty","Rate","Amount"]
[null," "]
[null,"TOTAL BROUGHT DOWN"]
[]
["H3.6","Inlet Cone"]
[null,"Supply and install fan inlet cone complete with bird proof wire mesh screen.","No",1]
[null,"Size: "]
[]
["H4","Extraction System (Storage)"]
[]
[null,"Supply, deliver and install the following items:"]
[]
["H4.1","Extraction Fan ","No",1]
[null,"Fan Type: Wall Mounted "]
[null,"Fan Make: ………...or equal and approved"]
[null,"Fan Size: …….diameter or ….x….."]
[null,"Process Data: Airflow (L/s) @ Pressure"]
[null,"Rotational Speed: ……….rpm"]
[null,"Mounting: Anti-Vibration Mounts, Ceiling/Wall mounting kit "]
[null,"Motor Size: (KW)"]
[]
["H4.2","Door Grille","No",1]
[null,"Make: "]
[null,"Size: "]
[null,"Finish: Epoxy Powder Coated, Aluminium Anodised or Standard colour to Arch's specification."]
[]
["H4.3","Control Box for fan to switch on when lights are operational.","No",1]
{"$rows_empty":21}
[null,"SUBTOTAL CARRIED FORWARD TO SUMMARY",{"$nulls":3},{"v":0,"d":"R 0.00"}]

{"sheet":"Ground Floor ","index":9,"n_rows":176,"n_cols":6,"rows_kept":176,"hidden":true,"flags":["formulas_cached_only"]}
["No","Description","Unit","Qty","Rate","Amount"]
["I","HVAC - Ground Floor "]
[]
["I1","Air-Conditioning "]
[]
["I1.1","Shop G002"]
[]
[null,"Chilled Water Fan-Coil Units (Hide-aways)"]
[]
[null,"Supply, installation and commissioning of high efficiency fan coil unit with, 2-pipe finned coil to provide cooling and electrical elements to provide electric heating as specified below c/w high efficiency EC fans and alluminium or copper air cooled fins."]
[]
[null,"Supply complete with solenoid valves, instrumentation, electrical equipment, wall mounted and fan coil mounted controller. Control to be integratable with BMS (by others) using Modbus, allowing the BMS operator to switch unit on/off, adjust set-point, and mode, and also to record fault signals"]
[]
["I1.1.1","Brand: Aermec, Trane, Sinko or similar approved","No",1]
[null,"Type: Hide-away "]
[null,"Cooling Capacity:    KW (Total)       KW (Sensible)"]
[null,"Heating capacity:    KW (Electric heating)"]
[null,"Supply airflow:     L/s (or better)"]
[]
["I1.1.2","Ducting - Un-insulated"]
[null,"Low Pressure Galvanised ducting including flexible connections, transformation pieces, bends, shoe pieces, spogots, stop ends and all duct fittings to SANS 1238, \"S\" slip & Drive Slip, 0.6mm ","Sqm"]
[null,"Category 1"]
[]
["I1.1.3","External duct insulation to SANS 10173, 25mm thick thermal insulation with aluminium foil vapour barrier (FRK)","Sqm"]
[]
["I1.1.4","Balancing Damper "]
[null,"Balancing Damper to suit duct, manual type, made of sheet metal","No",1]
[null,"Size: "]
[]
["I1.1.5","Flexible Duct - Externally insulated"]
[null,"Supply and install wire reinforced aluminium flexible ducting complete with clamps; duct sealant and fixings. 1 500mm long","No",1]
[null,"Diameter: "]
[]
["I1.1.6","Diffuser","No",1]
[null,"Brand:   or similar approved"]
[null,"Plenum or Collar"]
[null,"Size: "]
[null,"Finish: Epoxy Powder Coated or Standard colour"]
[]
["I1.1.7","Return Air Grille","No",1]
[null,"Make: "]
[null,"Type: Egg Crate, disc valve"]
[null,"Size: "]
[null,"Finish: Epoxy Powder Coated, Aluminium Anodised or Standard colour to Arch's specification."]
[null,"Opposed Blade Damper (OBD): Y/N"]
[null,"Return Air Filter Frame (RAFF): Y/N"]
[]
[]
[]
[]
[]
[null,"TOTAL CARRIED FORWARD"]
[]
["No","Description","Unit","Qty","Rate","Amount"]
[null," "]
[null,"TOTAL BROUGHT DOWN"]
[]
["I1.1.8","Insulated Condensate Drain","m",1]
[null,"Supply and install P-trapped uPVC drain piping including running joints, fittings, clamps, supports and connection to nearest drain point."]
[null,"Diameter: "]
[]
["I1.1.9","Stainless Steel Drip Tray","No",1]
[null,"Supply and install thermally insulated stainelss steel drip tray for the catment of any condensate from the valves."]
[null,"Size: "]
{"$rows_empty":11}
["I2","Extraction System "]
[]
[null,"Supply, deliver and install the following items:"]
[]
["I2.1","Extract Fan (Ablutions)","No",1]
[null,"Fan Type: In-line Axial Fan, Centrifugal Fan, Wall Mounted "]
[null,"Fan Make: ………...or equal and approved"]
[null,"Fan Size: …….diameter or ….x….."]
[null,"Process Data: Airflow (L/s) @ Pressure"]
[null,"Rotational Speed: ……….rpm"]
[null,"Mounting: Anti-Vibration Mounts, Ceiling/Wall mounting kit "]
[null,"Motor Size: (KW)"]
[]
["I2.2","Sound Attenuator","No",2]
[null,"Diameter to suit fan, with flexible collars"]
[null,"Length: 600L, 900L"]
[null,"POD type"]
[null,"NC rating: 35"]
[]
["I2.3","Weather Louver","No",1]
[null,"Make: ………...or equal and approved"]
[null,"Model:  ………...or equal and approved"]
[null,"Size: "]
[null,"Finish: Epoxy Powder Coated or Aluminium Anodised"]
[null,"Hinged with Washable pleated Filter"]
[]
["I2.4","Disc valves"]
[null,"Type: Extract air "]
[null,"Finish: Epoxy Powder Coated or Standard colour"]
[null,"Neck size: 100 mm dia","No",1]
[null,"Neck size: 150 mm dia","No",1]
[null,"Neck size: 200 mm dia","No",1]
[]
["I2.5","Door Grille","No",1]
[null,"Make: "]
[null,"Size: "]
[null,"Finish: Epoxy Powder Coated, Aluminium Anodised or Standard colour to Arch's specification."]
[]
[]
[]
[null,"TOTAL CARRIED FORWARD"]
[]
["No","Description","Unit","Qty","Rate","Amount"]
[null," "]
[null,"TOTAL BROUGHT DOWN"]
[]
["I2.6","Control Box for fan to switch on when lights are operational located in serrvice shaft or 24/7 timer.","No",1]
[]
["I2.7","Ducting"]
[null,"Low Pressure Galvanised ducting including flexible connections, transformation pieces, bends, shoe pieces, spogots, stop ends and all duct fittings to SANS 1238, \"S\" slip & Drive Slip, 0.6mm ","Sqm"]
[null,"Category 1"]
[]
["I2.8","Flexible Duct"]
[null,"Supply and install wire reinforced aluminium flexible ducting complete with clamps; duct sealant and fixings. 1 500 long","No",1]
[null,"Diameter: "]
[]
["I2.9","Balancing Damper "]
[null,"Balancing Damper to suit duct, manual type, made of sheet metal","No",1]
[null,"Size: "]
[]
["I2.10","Fire Damper "]
[null,"2 hour fire rated Fire Damper with Fusible Link or motorised ","No",1]
[null,"Size: "]
[]
["I3","Tempered Fresh Air System or Fans"]
{"$rows_empty":35}
[null,"SUBTOTAL CARRIED FORWARD TO SUMMARY",{"$nulls":3},{"v":0,"d":"R 0.00"}]

{"sheet":"First Floor ","index":10,"n_rows":158,"n_cols":6,"rows_kept":158,"hidden":true,"flags":["formulas_cached_only"]}
["No","Description","Unit","Qty","Rate","Amount"]
["J","HVAC - First Floor "]
[]
["J1","Air-Conditioning "]
[]
["J1.1","Shop F001"]
[]
[null,"Chilled Water Fan-Coil Units (Hide-aways)"]
[]
[null,"Supply, installation and commissioning of high efficiency fan coil unit with, 2-pipe finned coil to provide cooling and electrical elements to provide electric heating as specified below c/w high efficiency EC fans and alluminium or copper air cooled fins."]
[]
[null,"Supply complete with solenoid valves, instrumentation, electrical equipment, wall mounted and fan coil mounted controller. Control to be integratable with BMS (by others) using Modbus, allowing the BMS operator to switch unit on/off, adjust set-point, and mode, and also to record fault signals"]
[]
["J1.1.1","Brand: Aermec, Trane, Sinko or similar approved","No",1]
[null,"Type: Hide-away "]
[null,"Cooling Capacity:    KW (Total)       KW (Sensible)"]
[null,"Heating capacity:    KW (Electric heating)"]
[null,"Supply airflow:     L/s (or better)"]
[]
["J1.1.2","Ducting - Un-insulated"]
[null,"Low Pressure Galvanised ducting including flexible connections, transformation pieces, bends, shoe pieces, spogots, stop ends and all duct fittings to SANS 1238, \"S\" slip & Drive Slip, 0.6mm ","Sqm"]
[null,"Category 1"]
[]
["J1.1.3","External duct insulation to SANS 10173, 25mm thick thermal insulation with aluminium foil vapour barrier (FRK)","Sqm"]
[]
["J1.1.4","Balancing Damper "]
[null,"Balancing Damper to suit duct, manual type, made of sheet metal","No",1]
[null,"Size: "]
[]
["J1.1.5","Flexible Duct - Externally insulated"]
[null,"Supply and install wire reinforced aluminium flexible ducting complete with clamps; duct sealant and fixings. 1 500mm long","No",1]
[null,"Diameter: "]
[]
["J1.1.6","Diffuser","No",1]
[null,"Brand:   or similar approved"]
[null,"Plenum or Collar"]
[null,"Size: "]
[null,"Finish: Epoxy Powder Coated or Standard colour"]
[]
["J1.1.7","Return Air Grille","No",1]
[null,"Make: "]
[null,"Type: Egg Crate, disc valve"]
[null,"Size: "]
[null,"Finish: Epoxy Powder Coated, Aluminium Anodised or Standard colour to Arch's specification."]
[null,"Opposed Blade Damper (OBD): Y/N"]
[null,"Return Air Filter Frame (RAFF): Y/N"]
[]
[]
[]
[null,"TOTAL CARRIED FORWARD"]
[]
["No","Description","Unit","Qty","Rate","Amount"]
[null," "]
[null,"TOTAL BROUGHT DOWN"]
[]
["J1.1.8","Condensate Drain","m",1]
[null,"Supply and install P-trapped uPVC drain piping including running joints, fittings, clamps, supports and connection to nearest drain point."]
[null,"Diameter: "]
[]
["J1.1.9","Stainless Steel Drip Tray","No",1]
[null,"Supply and install thermally insulated stainelss steel drip tray for the catment of any condensate from the valves."]
[null,"Size: "]
[]
["J1.2","Shop F002"]
{"$rows_empty":7}
["J2","Extraction System "]
[]
[null,"Supply, deliver and install the following items:"]
[]
["J2.1","Extract Fan (Ablutions)","No",1]
[null,"Fan Type: In-line Axial Fan, Centrifugal Fan, Wall Mounted "]
[null,"Fan Make: ………...or equal and approved"]
[null,"Fan Size: …….diameter or ….x….."]
[null,"Process Data: Airflow (L/s) @ Pressure"]
[null,"Rotational Speed: ……….rpm"]
[null,"Mounting: Anti-Vibration Mounts, Ceiling/Wall mounting kit "]
[null,"Motor Size: (KW)"]
[]
["J2.2","Sound Attenuator","No",2]
[null,"Diameter to suit fan, with flexible collars"]
[null,"Length: 600L, 900L"]
[null,"POD type"]
[null,"NC rating: 35"]
[]
["J2.3","Weather Louver","No",1]
[null,"Make: ………...or equal and approved"]
[null,"Model:  ………...or equal and approved"]
[null,"Size: "]
[null,"Finish: Epoxy Powder Coated or Aluminium Anodised"]
[null,"Hinged with Washable pleated Filter"]
[]
["J2.4","Disc valves"]
[null,"Type: Extract air "]
[null,"Finish: Epoxy Powder Coated or Standard colour"]
[null,"Neck size: 100 mm dia","No",1]
[null,"Neck size: 150 mm dia","No",1]
[null,"Neck size: 200 mm dia","No",1]
[]
["J2.5","Door Grille","No",1]
[null,"Make: "]
[null,"Size: "]
[null,"Finish: Epoxy Powder Coated, Aluminium Anodised or Standard colour to Arch's specification."]
[]
[]
[]
[null,"TOTAL CARRIED FORWARD"]
[]
["No","Description","Unit","Qty","Rate","Amount"]
[null," "]
[null,"TOTAL BROUGHT DOWN"]
[]
["J2.6","Control Box for fan to switch on when lights are operational located in serrvice shaft or 24/7 timer.","No",1]
[]
["J2.7","Ducting"]
[null,"Low Pressure Galvanised ducting including flexible connections, transformation pieces, bends, shoe pieces, spogots, stop ends and all duct fittings to SANS 1238, \"S\" slip & Drive Slip, 0.6mm ","Sqm"]
[null,"Category 1"]
[]
["J2.8","Flexible Duct"]
[null,"Supply and install wire reinforced aluminium flexible ducting complete with clamps; duct sealant and fixings. 1 500 long","No",1]
[null,"Diameter: "]
[]
["J2.9","Balancing Damper "]
[null,"Balancing Damper to suit duct, manual type, made of sheet metal","No",1]
[null,"Size: "]
[]
["J2.10","Fire Damper "]
[null,"2 hour fire rated Fire Damper with Fusible Link or motorised ","No",1]
[null,"Size: "]
[]
["J3","Tempered Fresh Air System or Fans"]
{"$rows_empty":21}
[null,"SUBTOTAL CARRIED FORWARD TO SUMMARY",{"$nulls":3},{"v":0,"d":"R 0.00"}]