{"text_format":"3","workbook":"xls","n_sheets":16,"sheets":["Sheet2","Technical evaluation criter (2)","Technical evaluation criteria","Drop side load body 3500","Drop side load body 7000","Drop side load body 12000","Drop side load body 18000","Drop side load body 26000","6CUB Tipper","8CUB Tipper","10CUB Tipper","12CUB Tipper","Ply wood Tool Box","Wooden toolboxe lockable lids","Wooden toolboxes 8mm ply wood","Sheet1"],"not_rendered":{"images":26,"external_links":1,"comments":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet2","index":0,"n_rows":32,"n_cols":28,"rows_kept":32,"hidden":true,"flags":["formulas_cached_only"]}
[null,"AA Type canopy","Half Door Fibe Glass Canop","Fiberglas Canopy Can 4 ","F Glass Can  tilt-up side doors","Interframe with  drawer system ","Interframe with ladderrack","Single Ladder rack half length","Double ladder rack half length","PDC front bumper ","PDC Rear bumper ","LED Daytime running lamps","WORKING LIGHTS ","AMBER ROTATING LIGHT","Electrical","Electrical canopies","Roll Bar","SINGLE TOOLBOX ","LINK STICK HOLDERS","Ladder clamp","Ply wood Tool Box","Wooden  Side toolboxes","TOOLBOXES FOR 5 SEATER P VAN","Wooden toolboxe lockable lids","Wooden toolboxes 8mm ply wood","Wooden Floor and sides","Wooden Floor and Partition","PML"]
["L2 1600",null,"Half Door Fibe Glass Canop","Fiberglas Canopy Can 4 ","F Glass Can  tilt-up side doors","Interframe with  drawer system ","Interframe with ladderrack","Single Ladder rack half length","Double ladder rack half length","PDC front bumper ","PDC Rear bumper ","LED Daytime running lamps","WORKING LIGHTS ","AMBER ROTATING LIGHT","Electrical","Electrical canopies","Roll Bar","SINGLE TOOLBOX ","LINK STICK HOLDERS","Ladder clamp","Ply wood Tool Box","Wooden  Side toolboxes",null,"Wooden toolboxe lockable lids"]
["L2 B 1800",null,"Half Door Fibe Glass Canop","Fiberglas Canopy Can 4 ","F Glass Can  tilt-up side doors","Interframe with  drawer system ","Interframe with ladderrack","Single Ladder rack half length","Double ladder rack half length","PDC front bumper ","PDC Rear bumper ","LED Daytime running lamps","WORKING LIGHTS ","AMBER ROTATING LIGHT","Electrical","Electrical canopies","Roll Bar","SINGLE TOOLBOX ","LINK STICK HOLDERS","Ladder clamp","Ply wood Tool Box","Wooden  Side toolboxes",null,"Wooden toolboxe lockable lids"]
["L5",null,"Half Door Fibe Glass Canop","Fiberglas Canopy Can 4","F Glass Can  tilt-up side doors","Interframe with  drawer system ","Interframe with ladderrack","Single Ladder rack half length","Double ladder rack half length","PDC front bumper ","PDC Rear bumper ","LED Daytime running lamps","WORKING LIGHTS ","AMBER ROTATING LIGHT","Electrical","Electrical canopies","Roll Bar","SINGLE TOOLBOX ","LINK STICK HOLDERS","Ladder clamp","Ply wood Tool Box","Wooden  Side toolboxes",null,"Wooden toolboxe lockable lids"]
["L7","AA Type canopy","Half Door Fibe Glass Canop","Fiberglas Canopy Can 4","F Glass Can  tilt-up side doors","Interframe with  drawer system ","Interframe with ladderrack","Single Ladder rack half length","Double ladder rack half length","PDC front bumper ","PDC Rear bumper ","LED Daytime running lamps","WORKING LIGHTS ","AMBER ROTATING LIGHT","Electrical","Electrical canopies","Roll Bar","SINGLE TOOLBOX ","LINK STICK HOLDERS","Ladder clamp","Ply wood Tool Box","Wooden  Side toolboxes",null,"Wooden toolboxe lockable lids"]
["L8","AA Type canopy","Half Door Fibe Glass Canop","Fiberglas Canopy Can 4","F Glass Can  tilt-up side doors","Interframe with  drawer system ","Interframe with ladderrack","Single Ladder rack half length","Double ladder rack half length","PDC front bumper ","PDC Rear bumper ","LED Daytime running lamps","WORKING LIGHTS ","AMBER ROTATING LIGHT","Electrical","Electrical canopies","Roll Bar","SINGLE TOOLBOX ","LINK STICK HOLDERS","Ladder clamp","Ply wood Tool Box","Wooden  Side toolboxes",null,"Wooden toolboxe lockable lids"]
["L8D","AA Type canopy","Half Door Fibe Glass Canop","Fiberglas Canopy Can 4","F Glass Can  tilt-up side doors","Interframe with  drawer system ","Interframe with ladderrack","Single Ladder rack half length","Double ladder rack half length","PDC front bumper ","PDC Rear bumper ","LED Daytime running lamps","WORKING LIGHTS ","AMBER ROTATING LIGHT","Electrical","Electrical canopies","Roll Bar","SINGLE TOOLBOX ","LINK STICK HOLDERS","Ladder clamp","Ply wood Tool Box","Wooden  Side toolboxes",null,"Wooden toolboxe lockable lids"]
["L9","AA Type canopy","Half Door Fibe Glass Canop","Fiberglas Canopy Can 4","F Glass Can  tilt-up side doors","Interframe with  drawer system ","Interframe with ladderrack","Single Ladder rack half length","Double ladder rack half length","PDC front bumper ","PDC Rear bumper ","LED Daytime running lamps","WORKING LIGHTS ","AMBER ROTATING LIGHT","Electrical","Electrical canopies","Roll Bar","SINGLE TOOLBOX ","LINK STICK HOLDERS","Ladder clamp","Ply wood Tool Box","Wooden  Side toolboxes",null,"Wooden toolboxe lockable lids"]
["L9D","AA Type canopy","Half Door Fibe Glass Canop","Fiberglas Canopy Can 4","F Glass Can  tilt-up side doors","Interframe with  drawer system ","Interframe with ladderrack","Single Ladder rack half length","Double ladder rack half length","PDC front bumper ","PDC Rear bumper ","LED Daytime running lamps","WORKING LIGHTS ","AMBER ROTATING LIGHT","Electrical","Electrical canopies","Roll Bar","SINGLE TOOLBOX ","LINK STICK HOLDERS","Ladder clamp","Ply wood Tool Box","Wooden  Side toolboxes",null,"Wooden toolboxe lockable lids"]
["L11","AA Type canopy","Half Door Fibe Glass Canop","Fiberglas Canopy Can 4","F Glass Can  tilt-up side doors","Interframe with  drawer system ","Interframe with ladderrack","Single Ladder rack half length","Double ladder rack half length","PDC front bumper ","PDC Rear bumper ","LED Daytime running lamps","WORKING LIGHTS ","AMBER ROTATING LIGHT","Electrical","Electrical canopies","Roll Bar","SINGLE TOOLBOX ","LINK STICK HOLDERS","Ladder clamp","Ply wood Tool Box","Wooden  Side toolboxes",null,"Wooden toolboxe lockable lids"]
["L11D","AA Type canopy","Half Door Fibe Glass Canop","Fiberglas Canopy Can 4","F Glass Can  tilt-up side doors","Interframe with  drawer system ","Interframe with ladderrack","Single Ladder rack half length","Double ladder rack half length","PDC front bumper ","PDC Rear bumper ","LED Daytime running lamps","WORKING LIGHTS ","AMBER ROTATING LIGHT","Electrical","Electrical canopies","Roll Bar","SINGLE TOOLBOX ","LINK STICK HOLDERS","Ladder clamp","Ply wood Tool Box","Wooden  Side toolboxes",null,"Wooden toolboxe lockable lids"]
["L12","AA Type canopy","Half Door Fibe Glass Canop","Fiberglas Canopy Can 4","F Glass Can  tilt-up side doors","Interframe with  drawer system ","Interframe with ladderrack","Single Ladder rack half length","Double ladder rack half length","PDC front bumper ","PDC Rear bumper ","LED Daytime running lamps","WORKING LIGHTS ","AMBER ROTATING LIGHT","Electrical","Electrical canopies","Roll Bar","SINGLE TOOLBOX ","LINK STICK HOLDERS","Ladder clamp","Ply wood Tool Box","Wooden  Side toolboxes",null,"Wooden toolboxe lockable lids"]
["L12D","AA Type canopy","Half Door Fibe Glass Canop","Fiberglas Canopy Can 4","F Glass Can  tilt-up side doors","Interframe with  drawer system ","Interframe with ladderrack","Single Ladder rack half length","Double ladder rack half length","PDC front bumper ","PDC Rear bumper ","LED Daytime running lamps","WORKING LIGHTS ","AMBER ROTATING LIGHT","Electrical","Electrical canopies","Roll Bar","SINGLE TOOLBOX ","LINK STICK HOLDERS","Ladder clamp","Ply wood Tool Box","Wooden  Side toolboxes",null,"Wooden toolboxe lockable lids"]
["L13","AA Type canopy","Half Door Fibe Glass Canop","Fiberglas Canopy Can 4","F Glass Can  tilt-up side doors","Interframe with  drawer system ","Interframe with ladderrack","Single Ladder rack half length","Double ladder rack half length","PDC front bumper ","PDC Rear bumper ","LED Daytime running lamps","WORKING LIGHTS ","AMBER ROTATING LIGHT","Electrical","Electrical canopies","Roll Bar","SINGLE TOOLBOX ","LINK STICK HOLDERS","Ladder clamp","Ply wood Tool Box","Wooden  Side toolboxes",null,"Wooden toolboxe lockable lids",{"$nulls":3},"PML"]
["L13D","AA Type canopy","Half Door Fibe Glass Canop","Fiberglas Canopy Can 4","F Glass Can  tilt-up side doors","Interframe with  drawer system ","Interframe with ladderrack","Single Ladder rack half length","Double ladder rack half length","PDC front bumper ","PDC Rear bumper ","LED Daytime running lamps","WORKING LIGHTS ","AMBER ROTATING LIGHT","Electrical","Electrical canopies","Roll Bar","SINGLE TOOLBOX ","LINK STICK HOLDERS","Ladder clamp","Ply wood Tool Box","Wooden  Side toolboxes",null,"Wooden toolboxe lockable lids",{"$nulls":3},"PML"]
["L14 ","AA Type canopy","Half Door Fibe Glass Canop","Fiberglas Canopy Can 4","F Glass Can  tilt-up side doors","Interframe with  drawer system ","Interframe with ladderrack","Single Ladder rack half length","Double ladder rack half length","PDC front bumper ","PDC Rear bumper ","LED Daytime running lamps","WORKING LIGHTS ","AMBER ROTATING LIGHT","Electrical","Electrical canopies","Roll Bar","SINGLE TOOLBOX ","LINK STICK HOLDERS","Ladder clamp","Ply wood Tool Box","Wooden  Side toolboxes",null,"Wooden toolboxe lockable lids"]
["L14D","AA Type canopy","Half Door Fibe Glass Canop","Fiberglas Canopy Can 4","F Glass Can  tilt-up side doors","Interframe with  drawer system ","Interframe with ladderrack","Single Ladder rack half length","Double ladder rack half length","PDC front bumper ","PDC Rear bumper ","LED Daytime running lamps","WORKING LIGHTS ","AMBER ROTATING LIGHT","Electrical","Electrical canopies","Roll Bar","SINGLE TOOLBOX ","LINK STICK HOLDERS","Ladder clamp","Ply wood Tool Box","Wooden  Side toolboxes",null,"Wooden toolboxe lockable lids"]
["L15","AA Type canopy","Half Door Fibe Glass Canop","Fiberglas Canopy Can 4","F Glass Can  tilt-up side doors","Interframe with  drawer system ","Interframe with ladderrack","Single Ladder rack half length","Double ladder rack half length","PDC front bumper ","PDC Rear bumper ","LED Daytime running lamps","WORKING LIGHTS ","AMBER ROTATING LIGHT","Electrical","Electrical canopies","Roll Bar","SINGLE TOOLBOX ","LINK STICK HOLDERS","Ladder clamp","Ply wood Tool Box","Wooden  Side toolboxes",null,"Wooden toolboxe lockable lids"]
["L15D","AA Type canopy","Half Door Fibe Glass Canop","Fiberglas Canopy Can 4","F Glass Can  tilt-up side doors","Interframe with  drawer system ","Interframe with ladderrack","Single Ladder rack half length","Double ladder rack half length","PDC front bumper ","PDC Rear bumper ","LED Daytime running lamps","WORKING LIGHTS ","AMBER ROTATING LIGHT","Electrical","Electrical canopies","Roll Bar","SINGLE TOOLBOX ","LINK STICK HOLDERS","Ladder clamp","Ply wood Tool Box","Wooden  Side toolboxes",null,"Wooden toolboxe lockable lids"]
["L16D","AA Type canopy","Half Door Fibe Glass Canop","Fiberglas Canopy Can 4","F Glass Can  tilt-up side doors","Interframe with  drawer system ","Interframe with ladderrack","Single Ladder rack half length","Double ladder rack half length","PDC front bumper ","PDC Rear bumper ","LED Daytime running lamps","WORKING LIGHTS ","AMBER ROTATING LIGHT","Electrical","Electrical canopies","Roll Bar","SINGLE TOOLBOX ","LINK STICK HOLDERS","Ladder clamp","Ply wood Tool Box","Wooden  Side toolboxes",null,"Wooden toolboxe lockable lids"]
["L17D","AA Type canopy","Half Door Fibe Glass Canop","Fiberglas Canopy Can 4","F Glass Can  tilt-up side doors","Interframe with  drawer system ","Interframe with ladderrack","Single Ladder rack half length","Double ladder rack half length","PDC front bumper ","PDC Rear bumper ","LED Daytime running lamps","WORKING LIGHTS ","AMBER ROTATING LIGHT","Electrical","Electrical canopies","Roll Bar","SINGLE TOOLBOX ","LINK STICK HOLDERS","Ladder clamp","Ply wood Tool Box","Wooden  Side toolboxes",null,"Wooden toolboxe lockable lids"]
["L18D","AA Type canopy","Half Door Fibe Glass Canop","Fiberglas Canopy Can 4","F Glass Can  tilt-up side doors","Interframe with  drawer system ","Interframe with ladderrack","Single Ladder rack half length","Double ladder rack half length","PDC front bumper ","PDC Rear bumper ","LED Daytime running lamps","WORKING LIGHTS ","AMBER ROTATING LIGHT","Electrical","Electrical canopies","Roll Bar","SINGLE TOOLBOX ","LINK STICK HOLDERS","Ladder clamp","Ply wood Tool Box","Wooden  Side toolboxes",null,"Wooden toolboxe lockable lids"]
["L19D","AA Type canopy","Half Door Fibe Glass Canop","Fiberglas Canopy Can 4","F Glass Can  tilt-up side doors","Interframe with  drawer system ","Interframe with ladderrack","Single Ladder rack half length","Double ladder rack half length","PDC front bumper ","PDC Rear bumper ","LED Daytime running lamps","WORKING LIGHTS ","AMBER ROTATING LIGHT","Electrical","Electrical canopies","Roll Bar","SINGLE TOOLBOX ","LINK STICK HOLDERS","Ladder clamp","Ply wood Tool Box","Wooden  Side toolboxes",null,"Wooden toolboxe lockable lids"]
["L20D","AA Type canopy","Half Door Fibe Glass Canop","Fiberglas Canopy Can 4","F Glass Can  tilt-up side doors","Interframe with  drawer system ","Interframe with ladderrack","Single Ladder rack half length","Double ladder rack half length","PDC front bumper ","PDC Rear bumper ","LED Daytime running lamps","WORKING LIGHTS ","AMBER ROTATING LIGHT","Electrical","Electrical canopies","Roll Bar","SINGLE TOOLBOX ","LINK STICK HOLDERS","Ladder clamp","Ply wood Tool Box","Wooden  Side toolboxes",null,"Wooden toolboxe lockable lids"]
["L21D","AA Type canopy","Half Door Fibe Glass Canop","Fiberglas Canopy Can 4","F Glass Can  tilt-up side doors","Interframe with  drawer system ","Interframe with ladderrack","Single Ladder rack half length","Double ladder rack half length","PDC front bumper ","PDC Rear bumper ","LED Daytime running lamps","WORKING LIGHTS ","AMBER ROTATING LIGHT","Electrical","Electrical canopies","Roll Bar","SINGLE TOOLBOX ","LINK STICK HOLDERS","Ladder clamp","Ply wood Tool Box","Wooden  Side toolboxes",null,"Wooden toolboxe lockable lids"]
["M1",{"$nulls":8},"PDC front bumper ","PDC Rear bumper ","LED Daytime running lamps","WORKING LIGHTS ","AMBER ROTATING LIGHT","Electrical",{"$nulls":8},"Wooden toolboxe lockable lids"]
["M2",{"$nulls":8},"PDC front bumper ","PDC Rear bumper ","LED Daytime running lamps","WORKING LIGHTS ","AMBER ROTATING LIGHT","Electrical",{"$nulls":8},"Wooden toolboxe lockable lids"]
["M3",{"$nulls":8},"PDC front bumper ","PDC Rear bumper ","LED Daytime running lamps","WORKING LIGHTS ","AMBER ROTATING LIGHT","Electrical",{"$nulls":8},"Wooden toolboxe lockable lids"]
["M5",{"$nulls":8},"PDC front bumper ","PDC Rear bumper ","LED Daytime running lamps","WORKING LIGHTS ","AMBER ROTATING LIGHT","Electrical",{"$nulls":8},"Wooden toolboxe lockable lids"]
["P1",{"$nulls":8},"PDC front bumper ","PDC Rear bumper ","LED Daytime running lamps","WORKING LIGHTS ","AMBER ROTATING LIGHT","Electrical",{"$nulls":7},"TOOLBOXES FOR 5 SEATER P VAN","Wooden toolboxe lockable lids","Wooden toolboxes 8mm ply wood","Wooden Floor and sides","Wooden Floor and Partition"]
["P2",{"$nulls":8},"PDC front bumper ","PDC Rear bumper ","LED Daytime running lamps","WORKING LIGHTS ","AMBER ROTATING LIGHT","Electrical",{"$nulls":7},"TOOLBOXES FOR 5 SEATER P VAN","Wooden toolboxe lockable lids","Wooden toolboxes 8mm ply wood","Wooden Floor and sides","Wooden Floor and Partition"]
["CCP1",{"$nulls":8},"PDC front bumper ","PDC Rear bumper ","LED Daytime running lamps","WORKING LIGHTS ","AMBER ROTATING LIGHT","Electrical",{"$nulls":8},"Wooden toolboxe lockable lids"]

{"sheet":"Technical evaluation criter (2)","index":1,"n_rows":15,"n_cols":4,"rows_kept":15,"hidden":true,"flags":["formulas_cached_only"]}
[]
[]
[]
[]
[null,"Technical evaluation criteria"]
[null,"Technical specification ","Score in %","Total score in %"]
[null,"Annex 3 completed in Colum D with yes  or a no and in colum E provide proof of Compliance (Indicate where to validate in datasheets / brochures)or reason for  non-compliance",15]
[null,"For body builders and canopy builders ,drawings of the proposed product .Submit drawing  and weight calculations*.  (*truck only)                                                                                                                           For Auto Electrical work ,Wiring diagram for planned work with clear indication where they tap into vehicles wiring. Sumbit Drawings .",25]
[null,"For body builders and canopy builders ,Proof of registration as a MIB,  certificate to build and homologate this items tendered for.Submit certificate                                                                                                                           ",20]
[null,"Proof of existing maintenance and repair support structure network"]
[null,"Final Assembling and fitment  should be based in Cape Peninsula / East london area --Supply adress of premises where manufacturing and assmbly will be done.",20]
[null,"Product supporting network in the Cape coastal cluster, supply map of support network, with contact numbers of service agents,or copy of SLA with supporting componies (Submit copy of SLA)",20]
[{"$nulls":3},{"v":0.9,"d":"90%"}]
[]
[null,null,100]

{"sheet":"Technical evaluation criteria","index":2,"n_rows":20,"n_cols":5,"rows_kept":20,"flags":["formulas_cached_only"]}
[null,"Technical evaluation criteria:"]
[null," "]
[null,null,"YES","NO","weighting score"]
[null,"Annex 3 completed in Colum D with yes  or a no and in colum E provide proof of Compliance (Indicate where to validate in datasheets / brochures)or reason for  non-compliance and attach brochures for reference.",null,null,{"v":0.5,"d":"50%"}]
[null,"For Manufacturers and canopy builders ,drawings of the proposed product .Submit drawing  and weight calculations*.  (*truck only)                                                                                                                           For Auto Electrical work ,Wiring diagram for planned work with clear indication where they tap into vehicles wiring. Submit Drawings.  100% adherance to scope of work is expected. Non compliance will be regarded as non submission. 100% adherance to the statement of work is expected from drawings and wiring diagram. Failure to adhere will deem your drawings non compliant.",null,null,{"v":0.2,"d":"20%"}]
[null,"For Manufacturers and canopy builders ,Proof of registration as a valid MIB certificate to build and homologate this items tendered for. and currently MIB is the only registered body for body building as per the department of transport.                                                                                                                     ",null,null,{"v":0.1,"d":"10%"}]
[null,"Final Assembling and fitment  area. Supplier must provide address of premises where manufacturing and assembly will be done and it must be in a company letterhead. Inspection of premises  to check  for compliance will be conducted.  Insurance confirmation letter for the company must be provided. ",null,null,{"v":0.1,"d":"10%"}]
[null,"After sales support network  within Gauteng and include contact numbers of service agents and copy of SLA  (Submit copy of SLA). Atleast four Service providers based in Gauteng major cities.",null,null,"1 service provider 2%, 2 and above service providers 3% 4 and above  service providers 5% "]
[]
[]
[]
[null,"Specify Warranty period in months"]
[null,"Pre delivery inspection conducted on your premises "]
[null,"This technical submission shall be completed and returned with tender documents indicating how each of the technical critreria have been achieved with examples, and schematics where required."]
[null,"Proof of existing maintenance and repair support structure network"]
[]
[null,"Minimum threshold is hundred percent (91%)"]
[]
[null,"Mzodumo Mlanjeni  : OTS"]
[null,"Signature                  : "]

{"sheet":"Drop side load body 3500","index":3,"n_rows":24,"n_cols":5,"rows_kept":24,"hidden":true,"merged":[[2,2,2,3],[23,0,23,4]],"flags":["formulas_cached_only"]}
[]
[]
[null,"Annexure A3","Tendering Service Provider to complete",null,"Eskom technical team to complete"]
[null,"An drop side load body is designed to be fitted to a HCV chassis cab 3500GVM. It is further designed to accommodate a truck mounted crane rear or front mounted.","Comply","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["Dropsied Body","To be according to make and model with crane rear or front mounted."]
["Body width","2.5 m"]
["Dropsies","450 mm"]
["Floor","To be of medium‑duty construction."]
[null,"Runners to be 150 x 75 mm PF channel, extended with 1.2 m and boxed with a single braze for crane mounting front or rear in crane of crane mounting."]
[null,"Cross members to be 76 x 38 mm channels spaced at plus minus 400mm intervals."]
[null,"Side sills to be 100 x 50 mm PF channel"]
[null,"Floor to be 4 mm commercial quality, mild steel plates. All joints To be but welded on top of Cross member."]
[null,"Four of Turf hooks to be Fitted in floor that must be box Underneath, 3 x Turf locks on each side of load body."]
[null,"Side doors to be 3 mm commercial quality mild steel with inverted angle supported on top of each drop side door and doors lock with handles."]
[null,"Drop post 175 x 54 mm channel to be in place with a drop pin."]
[null,"Crane to be mounted at rear as close as possible to rear axle."]
[null,"Tailboard to be exact same spec as headboard."]
[null,"Body steps & grab handle fitted to left side for access to load body"]
[null,"Load body to be manufactured according to Original Equipment Manufacturer (OEM) Specifications."]
[null,"Side and rear retro-reflective material to be fitted to vehicles and load body. (Road traffic Act and Regulations No. 192A)"]
["Acceptance / Acceptance"]
["Name of Evaluator : ",null,"Signature :"]
["Name of Verifier",null,"Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom."]

{"sheet":"Drop side load body 7000","index":4,"n_rows":24,"n_cols":5,"rows_kept":24,"hidden":true,"merged":[[2,2,2,3],[23,0,23,4]],"flags":["formulas_cached_only"]}
[]
[]
[null,"Annexure A3","Tendering Service Provider to complete",null,"Eskom technical team to complete"]
[null,"An drop side load body is designed to be fitted to a HCV chassis cab 7000GVM. It is further designed to accommodate a truck mounted crane rear or front mounted.","Comply","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["Dropsied Body","To be according to make and model with crane rear or front mounted."]
["Body width","2.5 m"]
["Dropsies","450 mm"]
["Floor","To be of heavy‑duty construction."]
[null,"Runners to be 200 x 75 mm PF channel, extended with 1.2 m and boxed with a single braze for crane mounting front or rear."]
[null,"Cross members to be 76 x 38 mm channels spaced at plus minus 365 mm intervals."]
[null,"Side sills to be 100 x 50 mm PF channel"]
[null,"Floor to be 5 mm commercial quality, mild steel plates. All joints To be but welded on top of Cross member."]
[null,"Six of Turf hooks to be Fitted in floor that must be box Underneath, 3 x Turf locks on each side of load body."]
[null,"Side doors to be 3 mm commercial quality mild steel with inverted angle supported on top of each drop side door and doors lock with handles."]
[null,"Drop post 175 x 54 mm channel to be in place with a drop pin."]
[null,"Crane to be mounted at rear as close as possible to rear axle."]
[null,"Tailboard to be exact same spec as headboard."]
[null,"Body steps & grab handle fitted to left side for access to load body"]
[null,"Load body to be manufactured according to Original Equipment Manufacturer (OEM) Specifications."]
[null,"Side and rear retro-reflective material to be fitted to vehicles and load body. (Road traffic Act and Regulations No. 192A)"]
["Acceptance / Acceptance"]
["Name of Evaluator : ",null,"Signature :"]
["Name of Verifier",null,"Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom."]

{"sheet":"Drop side load body 12000","index":5,"n_rows":24,"n_cols":5,"rows_kept":24,"hidden":true,"merged":[[2,2,2,3],[23,0,23,4]],"flags":["formulas_cached_only"]}
[]
[]
[null,"Annexure A3","Tendering Service Provider to complete",null,"Eskom technical team to complete"]
[null,"An drop side load body is designed to be fitted to a HCV chassis cab 12000GVM. It is further designed to accommodate a truck mounted crane rear or front mounted.","Comply","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["Dropsied Body","To be according to make and model with crane rear or front mounted."]
["Body width","2.5 m"]
["Drop sides","450 mm"]
["Floor","To be of heavy‑duty construction."]
[null,"Runners to be 200 x 75 mm PF channel, extended with 1.2 m and boxed with a single braze for crane mounting front or rear."]
[null,"Cross members to be 76 x 38 mm channels spaced at plus minus 365 mm intervals."]
[null,"Side sills to be 100 x 50 mm PF channel"]
[null,"Floor to be 5 mm commercial quality, mild steel plates. All joints To be but welded on top of Cross member."]
[null,"Six of Turf hooks to be Fitted in floor that must be box Underneath, 3 x Turf locks on each side of load body."]
[null,"Side doors to be 3 mm commercial quality mild steel with inverted angle supported on top of each drop side door and doors lock with handles."]
[null,"Drop post 175 x 54 mm channel to be in place with a drop pin."]
[null,"Crane to be mounted at rear as close as possible to rear axle."]
[null,"Tailboard to be exact same spec as headboard."]
[null,"Body steps & grab handle fitted to left side for access to load body"]
[null,"Load body to be manufacturer according to Original Equipment Manufacturer (OEM) Specifications."]
[null,"Side and rear retro-reflective material to be fitted to vehicles and load body. (Road traffic Act and Regulations No. 192A)"]
["Acceptance / Acceptance"]
["Name of Evaluator : ",null,"Signature :"]
["Name of Verifier",null,"Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom."]

{"sheet":"Drop side load body 18000","index":6,"n_rows":24,"n_cols":5,"rows_kept":24,"hidden":true,"merged":[[2,2,2,3],[23,0,23,4]],"flags":["formulas_cached_only"]}
[]
[]
[null,"Annexure A3","Tendering Service Provider to complete",null,"Eskom technical team to complete"]
[null,"An drop side load body is designed to be fitted to a HCV chassis cab 18000GVM. It is further designed to accommodate a truck mounted crane rear or front mounted.","Comply","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["Drop side Body","To be according to make and model with crane rear or front mounted."]
["Body width","2.5 m"]
["Drop sides","450 mm"]
["Floor","To be of heavy‑duty construction."]
[null,"Runners to be 200 x 75 mm PF channel, extended with 1.2 m and boxed with a single braze for crane mounting front or rear."]
[null,"Cross members to be 76 x 38 mm channels spaced at plus minus 365 mm intervals."]
[null,"Side sills to be 100 x 50 mm PF channel"]
[null,"Floor to be 5 mm commercial quality, mild steel plates. All joints To be but welded on top of Cross member."]
[null,"Six of Turf hooks to be Fitted in floor that must be box Underneath, 3 x Turf locks on each side of load body."]
[null,"Side doors to be 3 mm commercial quality mild steel with inverted angle supported on top of each drop side door and doors lock with handles."]
[null,"Drop post 175 x 54 mm channel to be in place with a drop pin."]
[null,"Crane to be mounted at rear as close as possible to rear axle."]
[null,"Tailboard to be exact same spec as headboard."]
[null,"Body steps & grab handle fitted to left side for access to load body"]
[null,"Load body to be manufactured according to Original Equipment Manufacturer (OEM) Specifications."]
[null,"Side and rear retro-reflective material to be fitted to vehicles and load body. (Road traffic Act and Regulations No. 192A)"]
["Acceptance / Acceptance"]
["Name of Evaluator : ",null,"Signature :"]
["Name of Verifier",null,"Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom."]

{"sheet":"Drop side load body 26000","index":7,"n_rows":24,"n_cols":5,"rows_kept":24,"hidden":true,"merged":[[2,2,2,3],[23,0,23,4]],"flags":["formulas_cached_only"]}
[]
[]
[null,"Annexure A3","Tendering Service Provider to complete",null,"Eskom technical team to complete"]
[null,"An drop side load body is designed to be fitted to a HCV chassis cab 26000GVM. It is further designed to accommodate a truck mounted crane rear or front mounted.","Comply","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["Drop side Body","To be according to make and model with crane rear or front mounted."]
["Body width","2.5 m"]
["Drop sides","450 mm"]
["Floor","To be of heavy‑duty construction."]
[null,"Runners to be 200 x 75 mm PF channel, extended with 1.2 m and boxed with a single braze for crane mounting front or rear."]
[null,"Cross members to be 76 x 38 mm channels spaced at plus minus 365 mm intervals."]
[null,"Side sills to be 100 x 50 mm PF channel"]
[null,"Floor to be 5 mm commercial quality, mild steel plates. All joints To be but welded on top of Cross member."]
[null,"Six of Turf hooks to be Fitted in floor that must be box Underneath, 3 x Turf locks on each side of load body."]
[null,"Side doors to be 3 mm commercial quality mild steel with inverted angle supported on top of each drop side door and doors lock with handles."]
[null,"Drop post 175 x 54 mm channel to be in place with a drop pin."]
[null,"Crane to be mounted at rear as close as possible to rear axle."]
[null,"Tailboard to be exact same spec as headboard."]
[null,"Body steps & grab handle fitted to left side for access to load body"]
[null,"Load body to be manufactured according to Original Equipment Manufacturer (OEM) Specifications."]
[null,"Side and rear retro-reflective material to be fitted to vehicles and load body. (Road traffic Act and Regulations No. 192A)"]
["Acceptance / Acceptance"]
["Name of Evaluator : ",null,"Signature :"]
["Name of Verifier",null,"Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom."]

{"sheet":"6CUB Tipper","index":8,"n_rows":21,"n_cols":5,"rows_kept":21,"hidden":true,"merged":[[2,2,2,3],[20,0,20,4]],"flags":["formulas_cached_only"]}
[]
[]
[null,"Annexure A3","Tendering Service Provider to complete",null,"Eskom technical team to complete"]
[null,"An 6 CUB tipper load body is designed to be fitted to a HCV chassis cab 15000 GVM duel wheel application (4x2). It is further designed to tip the load to the rear of the vehicle","Comply","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["Dropsied Body","To be according to make and model "]
["Body width","Floor to be 6 mm commercial quality, mild steel plates. All joints To be welded on top of Cross member."]
["Dropsies","Sides to be 6 mm commercial quality, mild steel plates."]
["Floor","Load body to be of heavy‑duty construction."]
[null,"Runners to be 178 x 54 mm commercial quality, mild steel  "]
[null,"Cross members to be 100 x 50 mm commercial quality, mild steel "]
[null,"Cross members to be 350 mm apart"]
[null,"Hydraulic cylinder to tip load to mounted behind cab"]
[null,"Rear tipper bushes 80mm OD and 50 mm ID"]
[null,"Tipper tailgate to be automatic release"]
[null,"Mud flaps to be mounted at rear wheels"]
[null,"LED type taillights to be mounted in rear tail board"]
[null,"Side and rear retro-reflective material to be fitted to vehicles and load body. (Road traffic Act and Regulations No. 192A)"]
["Acceptance / Acceptance"]
["Name of Evaluator : ",null,"Signature :"]
["Name of Verifier",null,"Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom."]

{"sheet":"8CUB Tipper","index":9,"n_rows":21,"n_cols":5,"rows_kept":21,"hidden":true,"merged":[[2,2,2,3],[20,0,20,4]],"flags":["formulas_cached_only"]}
[]
[]
[null,"Annexure A3","Tendering Service Provider to complete",null,"Eskom technical team to complete"]
[null,"An 8 CUB tipper load body is designed to be fitted to a HCV chassis cab 15000 GVM duel wheel application (6x4). It is further designed to tip the load to the rear of the vehicle","Comply","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["Dropsied Body","To be according to make and model "]
["Body width","Floor to be 6 mm commercial quality, mild steel plates. All joints To be welded on top of Cross member."]
["Dropsies","Sides to be 6 mm commercial quality, mild steel plates."]
["Floor","Load body to be of heavy‑duty construction."]
[null,"Runners to be 178 x 54 mm commercial quality, mild steel  "]
[null,"Cross members to be 100 x 50 mm commercial quality, mild steel "]
[null,"Cross members to be 350 mm apart"]
[null,"Hydraulic cylinder to tip load to mounted behind cab"]
[null,"Rear tipper bushes 80mm OD and 50 mm ID"]
[null,"Tipper tailgate to be automatic release"]
[null,"Mud flaps to be mounted at rear wheels"]
[null,"LED type taillights to be mounted in rear tail board"]
[null,"Side and rear retro-reflective material to be fitted to vehicles and load body. (Road traffic Act and Regulations No. 192A)"]
["Acceptance / Acceptance"]
["Name of Evaluator : ",null,"Signature :"]
["Name of Verifier",null,"Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom."]

{"sheet":"10CUB Tipper","index":10,"n_rows":21,"n_cols":5,"rows_kept":21,"hidden":true,"merged":[[2,2,2,3],[20,0,20,4]],"flags":["formulas_cached_only"]}
[]
[]
[null,"Annexure A3","Tendering Service Provider to complete",null,"Eskom technical team to complete"]
[null,"An 10 CUB tipper load body is designed to be fitted to a HCV chassis cab 17000 GVM duel wheel application (6x4). It is further designed to tip the load to the rear of the vehicle","Comply","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["Dropsied Body","To be according to make and model "]
["Body width","Floor to be 8 mm commercial quality, mild steel plates. All joints To be welded on top of Cross member."]
["Dropsies","Sides to be 6 mm commercial quality, mild steel plates."]
["Floor","Load body to be of heavy‑duty construction."]
[null,"Runners to be 200 x 75 mm commercial quality, mild steel  "]
[null,"Cross members to be 100 x 50 mm commercial quality, mild steel "]
[null,"Cross members to be 350 mm apart"]
[null,"Hydraulic cylinder to tip load to mounted behind cab"]
[null,"Rear tipper bushes 110 mm OD and 75.5 mm ID"]
[null,"Tipper tailgate to be automatic release"]
[null,"Mud flaps to be mounted at rear wheels"]
[null,"LED type taillights to be mounted in rear tail board"]
[null,"Side and rear retro-reflective material to be fitted to vehicles and load body. (Road traffic Act and Regulations No. 192A)"]
["Acceptance / Acceptance"]
["Name of Evaluator : ",null,"Signature :"]
["Name of Verifier",null,"Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom."]

{"sheet":"12CUB Tipper","index":11,"n_rows":21,"n_cols":5,"rows_kept":21,"hidden":true,"merged":[[2,2,2,3],[20,0,20,4]],"flags":["formulas_cached_only"]}
[]
[]
[null,"Annexure A3","Tendering Service Provider to complete",null,"Eskom technical team to complete"]
[null,"An 12 CUB tipper load body is designed to be fitted to a HCV chassis cab 18000 GVM duel wheel application (6x4). It is further designed to tip the load to the rear of the vehicle","Comply","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["Dropsied Body","To be according to make and model "]
["Body width","Floor to be 8 mm commercial quality, mild steel plates. All joints To be welded on top of Cross member."]
["Dropsies","Sides to be 6 mm commercial quality, mild steel plates."]
["Floor","Load body to be of heavy‑duty construction."]
[null,"Runners to be 200 x 75 mm commercial quality, mild steel  "]
[null,"Cross members to be 100 x 50 mm commercial quality, mild steel "]
[null,"Cross members to be 350 mm apart"]
[null,"Hydraulic cylinder to tip load to mounted behind cab"]
[null,"Rear tipper bushes 110 mm OD and 75.5 mm ID"]
[null,"Tipper tailgate to be automatic release"]
[null,"Mud flaps to be mounted at rear wheels"]
[null,"LED type taillights to be mounted in rear tail board"]
[null,"Side and rear retro-reflective material to be fitted to vehicles and load body. (Road traffic Act and Regulations No. 192A)"]
["Acceptance / Acceptance"]
["Name of Evaluator : ",null,"Signature :"]
["Name of Verifier",null,"Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom."]

{"sheet":"Ply wood Tool Box","index":12,"n_rows":17,"n_cols":5,"rows_kept":17,"hidden":true,"merged":[[2,2,2,3],[16,0,16,4]],"flags":["formulas_cached_only"]}
[]
[]
[null,"Annexure A3","Tendering Service Provider to complete",null,"Eskom technical team to complete"]
["Description","wooden Toolbox no1","Comply","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["Specification ","Length =   (Full width of load body)"]
[null,"Width = 600mm"]
["Toolbox no1","Height = 400 mm"]
[null,"Toolbox and lid to be manufactured of 8mm industrial ply wood."]
[" ","All edges to be rounded off."]
[null,"Lid of tool box must be on top of toolbox."]
[null,"Lid must be lockable. (nose and staple)"]
[null,"Toolbox to be mounted on top of wooden floor and against wooden sides. All joints must be reinforced with solid wood strips / aluminium corner strips."]
[null,"The floor must be the full size of the load body floor and the sides must be up to the top of the load body sides. Manufactured of 8mm industrial ply wood. All wood must be sealed with a durable clear wood sealer."]
["Acceptance / Acceptance"]
["Name of Evaluator : ",null,"Signature :"]
["Name of Verifier",null,"Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom."]

{"sheet":"Wooden toolboxe lockable lids","index":13,"n_rows":23,"n_cols":5,"rows_kept":23,"hidden":true,"merged":[[2,2,2,3],[22,0,22,4]],"flags":["formulas_cached_only"]}
[]
[]
[null,"Annexure A3","Tendering Service Provider to complete",null,"Eskom technical team to complete"]
["Description","Wooden toolboxes with lockable lids, manufactured of 12mm industrial ply wood, mounted in back of Crew cab with wooden floor and sides. (1) Wooden partition between load area and crew area. (2) Two toolboxes on each side of load body.","Comply","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["Wooden Partition no1 ","Wooden partition made of 12 mm industrial ply = Full width and full height of load space directly behind the rear seat of the vehicle, with opening of 710mm X 400 mm in the middle – top part of the partition to access view for rear view mirror.  Opening must be covered with a metal grid."]
["                         Toolboxes no2","Toolboxes x 2, one on each side with 785 load space between tool boxes."]
[null,"Length =  ( From partition in front as far back as possible)"]
[null,"Width = 400mm"]
[null,"Height = 970 mm"]
[null,"Length = 950mm"]
["    ","Toolboxes and lids to be manufactured of 12mm industrial ply wood."]
[null,"All edges to be rounded off."]
[null,"Tool boxes must be made with loading space on top, full size of toolbox. Loading space in front left side = 3x pigeon holes 225x180 mm on top of each other. Cupboard with 2x doors opening side ways on the right side = 660mm x 530mm (doors =330 x 530) Cupboard on the bottom of the toolbox with lid opening to the bottom = 950mm x 280 mm."]
["Wooden floor and sides  ","Lids must be lockable. (nose and staple)"]
[null,"Toolboxes to be mounted on top of wooden floor and against wooden sides. Rear of toolboxes must follow the curve of the load space sides. All joints must be reinforced with solid wood strips / aluminium corner strips."]
[null,"The floor must be the full size of the load body floor and the sides must be up to the top of the toolbox back sides. Manufactured of 12mm industrial ply wood. All wood must be sealed with a durable clear wood sealer."]
["Loose tool box      ","Provision must be made for loose toolbox of 700x550x630mm with tie-down strap against back of partition."]
["Gas bottles ","Provision must be made for 2x gas bottles at the back of toolboxes with tie – down straps."]
["                             Comments","Outside corners of boxes must be reinforced with aluminium strips."]
["Acceptance / Acceptance"]
["Name of Evaluator : ",null,"Signature :"]
["Name of Verifier",null,"Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom."]

{"sheet":"Wooden toolboxes 8mm ply wood","index":14,"n_rows":20,"n_cols":5,"rows_kept":20,"hidden":true,"merged":[[2,2,2,3],[19,0,19,4]],"flags":["formulas_cached_only"]}
[]
[]
[null,"Annexure A3","Tendering Service Provider to complete",null,"Eskom technical team to complete"]
["Description","Wooden toolboxes with lockable lids, manufactured of 8mm industrial ply wood, mounted in canopy with wooden floor and sides. (1) Long toolbox across load body behind cab. (2) Two toolboxes on each side of load body.","Comply","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["Toolbox no1","Length =   (Full width of load body)"]
[null,"Width = 600mm"]
[null,"Height = 400 mm"]
["                         Toolboxes no2","Length =  ( From front tool box to as far back as possible)"]
[null,"Width = 350mm"]
[null,"Height = 400 mm"]
["    ","Toolboxes and lids to be manufactured of 8mm industrial ply wood."]
[null,"All edges to be rounded off."]
[null,"Lids of tool boxes must be on top of toolbox."]
[null,"Lids must be lockable. (nose and staple)"]
["  ","Toolboxes to be mounted on top of wooden floor and against wooden sides. All joints must be reinforced with solid wood strips / Aluminium corners strips."]
["Wooden floor and sides","The floor must be the full size of the load body floor and the sides must be up to the top of the load body sides. Manufactured of 8mm industrial ply wood. All wood must be sealed with a durable clear wood sealer."]
["Acceptance / Acceptance"]
["Name of Evaluator : ",null,"Signature :"]
["Name of Verifier",null,"Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom."]

{"sheet":"Sheet1","index":15,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}