{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":66,"n_cols":6,"rows_kept":66,"merged":[[0,4,0,5],[4,0,4,5],[65,0,65,4]],"flags":["formulas_cached_only"]}
["KOH Road Tanker Bund - Civil Works BOQ",{"$nulls":3},"2026-02-01"]
[]
["Bill of Quantities"]
["Item","Bill description","Unit","Bill quantity","Rate","Amount"]
["CIVIL & STRUCTURAL WORKS "]
[]
[]
["CONCRETE (STRUCTURAL)"]
[]
[1,"EXCAVATIONS"]
[]
["1.1.1","Excavate existing in-situ soils","m2",{"v":66,"d":"66.00"}]
[null,"Soft Excavation up to 1.5m, Cut to spoil "]
[]
["1.1.2","Compact existing in-situ soils under bund slab","m2",{"v":67,"d":"67.00"}]
[null,"to 95% Mod Aashto"]
[]
["2.1","FORMWORK"]
[]
["2.1.1","Vertical formwork for new max 1500mm high","m2",{"v":69,"d":"69.00"}]
[null,"bund walls with 25x25 corner chamfers"]
[]
["2.1.2","Vertical formwork for new sump inside bund","m2",{"v":1,"d":"1.00"}]
[]
[]
[]
["3.1","REINFORCEMENT"]
[]
["3.1.1","High Tensile Steel (Rate to include ordering from schedule, supply, delivered to site, fixed in position)"]
[]
["3.1.1.1","Y12, Y10 diameter bars - Bund","kg",{"v":2497,"d":"2,497"}]
[]
[]
[]
["4.1","CONCRETE"]
[]
[]
[4.1,"Reinforced Concrete"]
[]
["4.1.1","Concrete 25 MPa/19mm"]
[]
["4.1.1.1","Concrete bund walls max 1500mm high","m3",{"v":10,"d":"10.00"}]
[]
["4.1.1.2","Concrete bund floor, sump and ramp - 14,75m x 4,5m","m3",{"v":16,"d":"16.00"}]
[]
[]
[]
[]
[5.1,"STEELWORK"]
[]
["5.1.1","Sump frame, cast in 50x50x5 galvanized","m",{"v":1,"d":"1.00"}]
[null,"angles with fish tail lugs"]
[]
["5.1.2","Sump grating cover, galvanized","m2",{"v":0.3,"d":"0.30"}]
[null,"Mentis RS40x4.5"]
[]
["5.1.3","M12 chemical anchors","No",{"v":8,"d":"8.00"}]
[]
[]
[5.1,"MISCELANEOUS WORKS"]
[]
["5.1.1","Bund floor and bund walls inside area ","m2",{"v":72,"d":"72.00"}]
[null,"acid resistant epoxy flooring paint"]
[]
[]
["TOTAL"]