{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Bingoma"],"read":"whole","date_system":"1900"}

{"sheet":"Bingoma","index":0,"n_rows":2374,"n_cols":10,"rows_kept":2374,"merged":[[1011,0,1011,5],[1278,0,1278,5],[1506,0,1506,5],[1767,0,1767,5],[2005,0,2005,5],[2132,0,2132,5],[2188,0,2188,5],[2302,0,2302,5]]}
["."]
[]
["ITEM NO","DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT"]
[null,"SECTION 1","H1","0.0"]
[]
[null,"PRELIMINARIES","H1","0.0"]
[]
[null,"MEANING OF TERMS \"TENDER / TENDERER\"","H2","0.0"]
[]
[null,"Any reference to the words \"Tender\" or \"Tenderer\" herein and/or in any other documentation shall be construed to have the same meaning as the words \"Bid\" or \"Bidder\"",null,"0.0"]
[]
[null,"PRELIMINARIES","H2","0.0"]
[]
[null,"The JBCC Preliminaries Code 2103, May 2005 edition for use with the JBCC Principal Building Agreement Edition 4.1 Code 2101, March 2005 is taken to be incorporated herein. The tenderer is deemed to have referred to these documents for the full intent and meaning of each clause. These clauses are referred to by number and heading only. Where standard clauses or options are not applicable to the contract such modifications or corrections as are necessary are given under each relevant clause. Where an item is not relevant to this specific contract such item is marked. \"N/A\" signifying \"Not Applicable\".",null,"0.0"]
[]
[null,"PRICING OF PRELIMINARIES","H2","0.0"]
[]
[null,"Should Option A, as set out in clause B10.3.1 hereinafter be used for the adjustment of preliminaries then each item priced is to be allocated to one or more of the three categories Fixed, Value Related or Time Related and the respective amounts entered in the spaces provided under each item",null,"0.0"]
[]
[null,"Items not priced in these Preliminaries shall be deemed to be included elsewhere in these Bills of Quantities.",null,"0.0"]
[]
[null,"SECTION A: JBCC PRINCIPAL BUILDING AGREEMENT","H2","0.0"]
[]
[null,"DEFINITIONS","H2","0.0"]
[]
[null,"A1.0    DEFINITIONS AND INTERPRETATION Clause 1.0  Clause 1.1 Definition of \"Commencement Date\" is added:"]
[]
[null,"COMMENCEMENT DATE means the date that the agreement, made in terms of the Form of Offer and Acceptance, comes into effect"]
[]
[null,"Clause 1.1 Definition of \"Construction Guarantee\" is amended by replacing it with the following:"]
[]
[null,"CONSTRUCTION GUARANTEE means a guarantee at call obtained by the contractor from an institution approved by the employer in terms of the employer's construction guarantee form as selected in the schedule"]
[]
[null,"Clause 1.1 Definition of \"Construction Period\" is amended by replacing it with the following:"]
[]
[null,"CONSTRUCTION PERIOD means the period commencing on the commencement date and ending on the date of practical completion"]
[]
[null,"Clause 1.1 Definition of \"Corrupt Practice\" is added:"]
[]
[null,"CORRUPT PRACTICE means the offering, giving, receiving or soliciting of anything of value to influence the action of a public official in the procurement process or in contract execution"]
[]
[null,"Clause 1.1 Definition of \"Fraudulent Practice\" is added:"]
[]
[null,"FRAUDULENT PRACTICE means a misrepresentation of facts in order to influence a procurement process or the execution of a contract to the detriment of any tenderer and includes collusive practice among tenderers (prior to or after the tender submission) designed to establish tender prices at artificial non-competitive levels and to deprive the tenderer of the benefits of free and open competition"]
[]
[null,"Clause 1.1 Definition of \"Interest\" is amended by replacing it with the following:"]
[]
[null,"INTEREST means the interest rates applicable on this contract, whether specifically indicated in the relevant clauses or not, will be the rate as determined by the Minister of Finance, from time to time, in terms of section 80(1)(b) of the Public Finance Management Act, 1999 (Act No. 1 of 1999)"]
[]
[null,"Clause 1.1 Definition of \"Principal Agent\" is amended by replacing it with the following:"]
[]
[null,"PRINCIPAL AGENT means the person or entity appointed by the employer and named in the schedule. In the event of a principal agent not being appointed, then all the duties and obligations of a principal agent as detailed in the agreement shall be fulfilled by a representative of the employer as named in the schedule"]
[]
[null,"Clause 1.1 Definition of \"Security\" is amended by replacing it with the following:"]
[]
[null,"SECURITY means the form of security provided by the employer or contractor, as stated in the schedule, from which the contractor or employer may recover expense or loss"]
[]
[null,"Clause 1.6 is amended by replacing the words \"prepaid registered post, telefax or e-mail\" with \"prepaid registered post or telefax\""]
[]
[null,"Clause 1.6.4 is amended by replacing it with the following:"]
[]
[null,"No clause  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"OBJECTIVE AND PREPARATION"]
[]
[null,"A2.0 OFFER, ACCEPTANCE AND PERFORMANCE  Clause 2.0  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"A3.0 DOCUMENTS  Clause 3.0Clause 3.2.1 is amended by replacing\"14.1\" with \"14.0\"Clause 3.7 is amended by the addition of the following:  The contractor shall supply and keep a copy of the JBCC Series 2000 Principal Building Agreement and Preliminaries applicable to this contract on the site, to which the employer, principal agent and agents shall have access at all times Clause 3.10 is amended by replacing the second reference to \"principal agent\" with the word \"employer\" Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[null,"A4.0 DESIGN RESPONSIBILITY  Clause 4.0Clause 4.3 is amended by replacing it with the following: No clause Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[null,"A5.0 EMPLOYER'S AGENTS Clause 5.0 Clause 5.1.2 is amended to include clauses 32.6.3, 34.3, 34.4 and 38.5.8 Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"A6.0 SITE REPRESENTATIVE Clause 6.0 Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"A7.0 COMPLIANCE WITH REGULATIONS Clause 7.0 Note: A separate clause has been included in Section C : Specific Preliminaries of the bills of quantities / lump sum document for the contractor to have the opportunity to price for all the requirements of the Occupational Health and Safety Act, Construction Regulations and Health and Safety Specification Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"A8.0 WORKS RISK Clause 8.0 Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"A9.0 INDEMNITIES Clause 9.0 Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"A10.0 WORKS INSURANCES Clause 10.0 Clause 10.0 is amended by the addition of the following clauses:"]
[]
[null,"10.5 Damage to the Works  (a) Without in any way limiting the contractor's obligations in terms of the contract, the contractor shall bear the full risk of damage to and/or destruction of the works by whatever cause during construction of the works and hereby indemnifies and holds harmless the employer against any such damage. The contractor shall take such precautions and security measures and other steps for the protection and security of the works as the contractor may deem necessary"]
[]
[null,"(b) The contractor shall at all times proceed immediately to remove or dispose of any debris arising from damage to or destruction of the works and to rebuild, restore, replace and/or repair the works"]
[]
[null,"© The employer shall carry the risk of damage to or destruction of the works and materials paid for by the employer that is the result of the excepted risks as set out in 10.6"]
[]
[null,"(d) Where the employer bears the risk in terms of this contract, the contractor shall, if requested to do so, reinstate any damage or destroyed portions of the works and the costs of such reinstatement shall be measured and valued in terms of 32.0 hereof"]
[]
[null,"10.6 Injury to Persons or loss of or damage to Properties  (a) The contractor shall be liable for and hereby indemnifies the employer against any liability, loss, claim or proceeding whether arising in common law or by statute, consequent upon personal injuries to or the death of any person whomsoever arising out of or in the course of or caused by the execution of the works unless due to any act or negligence of any person for whose actions the employer is legally liable"]
[]
[null,"(b) The contractor shall be liable for and hereby indemnifies the employer against any liability, loss, claim or proceeding consequent upon loss of or damage to any moveable or immovable or personal property or property contiguous to the site, whether belonging to or under the control of the employer or any other body or person, arising out of or in the course of or by reason of the execution of the works unless due to any act or negligence of any person for whose actions the employer is legally liable"]
[]
[null,"© The contractor shall, upon receiving a contract instruction from the principal agent, cause the same to be made good in a perfect and workmanlike manner at his own cost and in default thereof the employer shall be entitled to cause it to be made good and to recover the cost thereof from the contractor or to deduct the same from amounts due to the contractor"]
[]
[null,"(d) The contractor shall be responsible for the protection and safety of such portions of the premises placed under his control by the employer for the purpose of executing the works until the issue of the certificate of practical completion"]
[]
[null,"(e )Where the execution of the works involves the risk of removal of or interference with support to adjoining properties including land or structures or any structures to be altered or added to, the contractor shall obtain adequate insurance and will remain adequately insured or insured to the specific limit stated in the contract against the death of or injury to persons or damage to such property consequent on such removal or interference with the support until such portion of the works has been completed"]
[]
[null,"(f) The contractor shall at all times proceed immediately at his own cost to remove or dispose of any debris and to rebuild, restore, replace and/or repair such property and to execute the works"]
[]
[null,"10.7 High risk insurance In the event of the project being executed in a geological area classified as a \"High Risk Area\", that is an area which is subject to highly unstable subsurface conditions that might result in catastrophic ground movement evident by sinkhole or doline formation the following will apply:"]
[]
[null,"10.7.1 Damage to the works  The contractor shall, from the commencement date of the works until the date of the certificate of practical completion bear the full risk of and hereby indemnifies and holds harmless the employer against any damage to and/or destruction of the works consequent upon a catastrophic ground movement as mentioned above. The contractor shall take such precautions and security measures and other steps for the protection of the works as he may deem necessary"]
[]
[null,"When so instructed to do so by the principal agent, the contractor shall proceed immediately to remove and/or dispose of any debris arising from damage to or destruction of the works and to rebuild, restore, replace and/or repair the works, at the contractor's own costs"]
[]
[null,"10.7.2 Injury to persons or loss of or damage to property  The contractor shall be liable for and hereby indemnifies and holds harmless the employer against any liability, loss, claim or proceeding arising at any time during the period of the contract whether arising in common law or by statute, consequent upon personal injuries to or the death of any person whomsoever resulting from, arising out of, or caused by a catastrophic ground movement as mentioned above"]
[]
[null,"The contractor shall be liable for and hereby indemnifies the employer against any and all liability, loss, claim or proceeding consequent upon loss of or damage to any moveable or immovable or personal property or property contiguous to the site, whether belonging to or under the control of the employer or any other body or person whomsoever arising out of or caused by a catastrophic ground movement, as mentioned above, which occurred during the period of the contract"]
[]
[null,"10.7.3 It is the responsibility of the contractor to ensure that he has adequate insurance to cover his risk and liability as mentioned in 10.7.1 and 10.7.2. Without limiting the contractor's obligations in terms of the contract, the contractor shall, within twenty-one (21) calendar days of the commencement date but before commencement of the works, submit to the employer proof of such insurance policy, if requested to do so"]
[]
[null,"10.7.4 The employer shall be entitled to recover any and all losses and/or damages of whatever nature suffered or incurred consequent upon the contractor's default of his obligations as set out in 10.7.1; 10.7.2 and 10.7.3. Such losses or damages may be recovered from the contractor or by deducting the same from any amounts still due under this contract or under any other contract presently or hereafter existing between the employer and the contractor and for this purpose all these contracts shall be considered one indivisible whole Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"A11.0 LIABILITY INSURANCES  Clause 11.0  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"A12.0 EFFECTING INSURANCES  Clause 12.0  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"A13.0 No clause N/A"]
[]
[null,"A14.0 SECURITY  Clause 14.0  Clauses 14.1 - 14.8 are amended by replacing them with the following:"]
[]
[null,"14.1 In respect of contracts with a contract sum up to R1 million, the security to be provided by the contractor to the employer will be a payment reduction of five per cent (5%) of the value certified in the payment certificate (excluding VAT)"]
[]
[null,"14.1.1 The payment reduction of the value certified in a payment certificate shall be mutatis mutandi in terms of 31.8(A)"]
[]
[null,"14.1.2 The employer shall be entitled to recover expense and loss from the payment reduction in terms of 33.0 provided that the employer complies with the provisions of 33.4 in which event the employer's entitlement shall take precedence over his obligations to refund the payment reduction security or portions thereof to the contractor"]
[]
[null,"14.2 In respect of contracts with a contract sum above R1 million, the contractor shall have the right to select the security to be provided in terms of 14.3, 14.4, 14.5, 14.6, or 14.7 as stated in the schedule. Such security shall be provided to the employer within twenty-one (21) calendar days from commencement date. Should the contractor fail to select the security to be provided or should the contractor fail to provide the employer with the selected security within twenty-one (21) calendar days from commencement date, the security in terms of 14.7 shall be deemed to have been selected"]
[]
[null,"14.3 Where security as a cash deposit of ten per cent (10%) of the contract sum (excluding VAT) has been selected:"]
[]
[null,"14.3.1 The contractor shall furnish the employer with a cash deposit equal in value to ten per cent (10%) of the contract sum (excluding VAT) within twenty-one (21) calendar days from commencement date"]
[]
[null,"14.3.2 Within twenty-one (21) calendar days of the date of practical completion of the works the employer shall reduce the cash deposit to an amount equal to three per cent (3%) of the contract value (excluding VAT), and refund the balance to the contractor"]
[]
[null,"14.3.3 Within twenty-one (21) calendar days of the date of final completion of the works the employer shall reduce the cash deposit to an amount equal to one per cent (1%) of the contract value (excluding VAT) and refund the balance to the contractor"]
[]
[null,"14.3.4 On the date of payment of the amount in the final payment certificate, the employer shall refund the remainder of the cash deposit to the contractor"]
[]
[null,"14.3.5 The employer shall be entitled to recover expense and loss from the cash deposit in terms of 33.0 provided that the employer complies with the provisions of 33.4 in which event the employer's entitlement shall take precedence over his obligations to refund the cash deposit security or portions thereof to the contractor"]
[]
[null,"14.3.6 The parties expressly agree that neither the employer nor the contractor shall be entitled to cede the rights to the deposit to any third party"]
[]
[null,"14.4 Where security as a variable construction guarantee of ten percent (10%) of the contract sum (excluding VAT) has been selected:"]
[]
[null,"14.4.1 The contractor shall furnish the employer with an acceptable variable construction guarantee equal in value to ten per cent (10%) of the contract sum (excluding VAT) within twenty-one (21) calendar days from commencement date"]
[]
[null,"14.4.2 The variable construction guarantee shall reduce and expire in terms of the Variable Construction Guarantee form included in the invitation to tender"]
[]
[null,"14.4.3 The employer shall return the variable construction guarantee to the contractor within fourteen (14) calendar days of it expiring"]
[]
[null,"14.4.4 Where the employer has a right of recovery against the contractor in terms of 33.0, the employer shall issue a written demand in terms of the variable construction guarantee"]
[]
[null,"14.5 Where security as a fixed construction guarantee of five per cent (5%) of the contract sum (excluding VAT) and a five per cent (5%) payment reduction of the value certified in the payment certificate (excluding VAT) has been selected:"]
[]
[null,"14.5.1 The contractor shall furnish a fixed construction guarantee to the employer equal in value to five per cent (5%) of the contract sum (excluding VAT)"]
[]
[null,"14.5.2 The fixed construction guarantee shall come into force on the date of issue and shall expire on the date of the last certificate of practical completion"]
[]
[null,"14.5.3 The employer shall return the fixed construction guarantee to the contractor within fourteen (14) calendar days of it expiring"]
[]
[null,"14.5.4 The payment reduction of the value certified in a payment certificate shall be in terms of 31.8 (A) and 34.8"]
[]
[null,"14.5.5 Where the employer has a right of recovery against the contractor in terms of 33.0, the employer shall be entitled to issue a written demand in terms of the fixed construction guarantee or may recover from the payment reduction or may do both"]
[]
[null,"14.6 Where security as a cash deposit of five per cent (5%) of the contract sum (excluding VAT) and a payment reduction of five per cent (5%) of the value certified in the payment certificate (excluding VAT) has been selected:"]
[]
[null,"14.6.1 The contractor shall furnish the employer with a cash deposit equal in value to five per cent (5%) of the contract sum (excluding VAT) within twenty-one (21) calendar days from commencement date"]
[]
[null,"14.6.2 Within twenty-one (21) calendar days of the date of practical completion of the works the employer shall refund the cash deposit in total to the contractor"]
[]
[null,"14.6.3 The payment reduction of the value certified in a payment certificate shall be mutatis mutandi in terms of 31.8(A)"]
[]
[null,"14.6.4 Where the employer has a right of recovery against the contractor in terms of 33.0, the employer may issue a written notice in terms of 33.4 or may recover from the payment reduction or may do both"]
[]
[null,"14.7 Where security as a payment reduction of ten per cent (10%) of the value certified in the payment certificate (excluding VAT) has been selected:"]
[]
[null,"14.7.1 The payment reduction of the value certified in a payment certificate shall be mutatis mutandi in terms of 31.8(B)"]
[]
[null,"14.7.2 The employer shall be entitled to recover expense and loss from the payment reduction in terms of 33.0 provided that the employer complies with the provisions of 33.4 in which event the employer's entitlement shall take precedence over his obligations to refund the payment reduction or portions thereof to the contractor"]
[]
[null,"14.8 Payments made by the guarantor to the employer in terms of the fixed or variable construction guarantee shall not prejudice the rights of the employer or contractor in terms of this agreement"]
[]
[null,"14.9 Should the contractor fail to furnish the security in terms of 14.2, the employer, in his sole discretion and without notification to the contractor, is entitled to change the contractor's selected form of security to that of a ten per cent (10%) payment reduction of the value certified in the payment certificate (excluding VAT), whereafter 14.7 shall be applicable  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"EXECUTION"]
[]
[null,"A15.0 PREPARATION FOR AND EXECUTION OF THE WORKS  Clause 15.0  Clause 15.1.1 is amended by replacing it with:  No clause  Clause 15.1.2 is amended by replacing it with:  The security selected in terms of 14.0"]
[]
[null,"Clause 15.1 is amended by the addition of the following clause:  15.1.4 An acceptable health and safety plan, required in terms of the Occupational Health and Safety Act, 1993 (Act 85 of 1993), within twenty-one (21) calendar days of commencement date"]
[]
[null,"Clause 15.2.1 is amended by replacing it with the following clause:"]
[]
[null,"Give the contractor possession of the site within ten (10) working days of the contractor complying with the terms of 15.1.4  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"A16.0 ACCESS TO THE WORKS  Clause 16.0  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"A17.0 CONTRACT INSTRUCTIONS  Clause 17.0  Clause 17.1.11 is amended by deleting the words \"and the appointment of nominated and selected subcontractors\"  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"A18.0 SETTING OUT OF THE WORKS  Clause 18.0  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"A19.0 ASSIGNMENT  Clause 19.0  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"A20.0 NOMINATED SUBCONTRACTORS  Clause 20.0  Clause 20.1.3 is amended by replacing it with the following:  No clause  Note: See item B9.1 hereinafter for adjustment of attendance on nominated subcontractors executing work allowed for under provisional sums  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"A21.0 SELECTED SUBCONTRACTORS  Clause 21.0  Clause 21 is amended by replacing it with:  No clause  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"A22.0 EMPLOYER'S DIRECT CONTRACTORS  Clause 22.0  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"A23.0 CONTRACTOR'S DOMESTIC SUBCONTRACTORS  Clause 23.0  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"COMPLETION"]
[]
[null,"A24.0 PRACTICAL COMPLETION  Clause 24.0  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"A25.0 WORKS COMPLETION  Clause 25.0  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"A26.0 FINAL COMPLETION  Clause 26.0  Clause 26.1.2 is amended by inserting \"#\" next to 26.1.2  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"A27.0 LATENT DEFECTS LIABILITY PERIOD  Clause 27.0  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"A28.0 SECTIONAL COMPLETION  Clause 28.0  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"A29.0 REVISION OF DATE FOR PRACTICAL COMPLETION  Clause 29.0  Clause 29.2.5 is amended by replacing it with:  No clause  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"A30.0 PENALTY FOR NON-COMPLETION  Clause 30.0  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"PAYMENT"]
[]
[null,"A31.0 INTERIM PAYMENT TO THE CONTRACTOR  Clause 31.0"]
[]
[null,"Clause 31.5.2 is amended by replacing \"14.7.1\" with \"14.0\""]
[]
[null,"Clause 31.8 is amended by replacing it with the following two alternative clauses:"]
[]
[null,"Alternative A  31.8(A) Where a security is selected in terms of 14.1; 14.5 or 14.6, the value of the works in terms of 31.4.1 and materials and goods in terms of 31.4.2 shall be certified in full. The value certified shall be subject to the following percentage adjustments:"]
[]
[null,"31.8(A).1 Ninety-five per cent (95%) of such value in interim payment certificates issued up to the date of practical completion"]
[]
[null,"31.8(A).2 Ninety-seven per cent (97%) of such value in interim payment certificates issued on the date of practical completion and up to but excluding the date of final completion"]
[]
[null,"31.8(A).3 Ninety-nine per cent (99%) of such value in interim payment certificates issued on the date of final completion and up to but excluding the final payment certificate in terms of 34.6"]
[]
[null,"31.8(A).4 One hundred per cent (100%) of such value in the final payment certificate in terms of 34.6 except where the amount certified is in favour of the employer. In such an event the payment reduction shall remain at the adjustment level applicable to the final payment certificate"]
[]
[null,"Alternative B"]
[]
[null,"31.8(B) Where security as a payment reduction in terms of 14.7 has been selected, the value of the works in terms of 31.4.1 and materials and goods in terms of 31.4.2 shall be certified in full. The value certified shall be subject to the following percentage adjustments:"]
[]
[null,"31.8(B).1 Ninety per cent (90%) of such value in interim payment certificates issued up to the date of practical completion"]
[]
[null,"31.8(B).2 Ninety-seven per cent (97%) of such value in interim payment certificates issued on the date of practical completion and up to but excluding the date of final completion"]
[]
[null,"31.8(B).3 Ninety-nine per cent (99%) of such value in interim payment certificates issued on the date of final completion and up to but excluding the final payment certificate in terms of 34.6"]
[]
[null,"31.8(B).4 One hundred per cent (100%) of such value in the final payment certificate in terms of 34.6 except where the amount certified is in favour of the employer. In such an event the payment reduction shall remain at the adjustment level applicable to the final payment certificate"]
[]
[null,"Clause 31.12 is amended by deleting the following:"]
[]
[null,"Payment shall be subject to the employer giving the contractor a tax invoice for the amount due  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"A32.0 ADJUSTMENT TO THE CONTRACT VALUE  Clause 32.0  Clauses 32.5.1, 32.5.4 and 32.5.7 are amended by the addition of the following at the end of the sentence:  \"due to no fault of the contractor\"  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"A33.0 RECOVERY OF EXPENSE AND LOSS  Clause 33.0  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"A34.0 FINAL ACCOUNT AND FINAL PAYMENT  Clause 34.0  Clause 34.1 is amended by removing \"#\" next to 34.1  Clause 34.2 is amended by inserting \"#\" next to 34.2  Clause 34.8 is amended by deleting the words \"where security as a fixed construction guarantee in terms of 14.4 has been selected or where payment reduction has been applied in terms of 14.7.1\"  Clause 34.13 is amended by replacing \"seven (7) calendar days\" with \"twenty-one (21) calendar days\" and deleting the words \"subject to the employer giving the contractor a tax invoice for the amount due\"  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"A35.0 PAYMENT TO OTHER PARTIES  Clause 35.0  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"CANCELLATION"]
[]
[null,"A36.0 CANCELLATION BY EMPLOYER - CONTRACTOR'S DEFAULT   Clause 36.0  Clause 36.1 is amended by the addition of the following clauses:  36.1.3 refuses or neglects to comply strictly with any of the conditions of contract  36.1.4 estate being sequestrated, liquidated or surrendered in terms of the insolvency laws in force within the Republic of South Africa  36.1.5 in the judgement of the employer, has engaged in corrupt or fraudulent practices in competing for or in executing the contract  Clause 36.3 is amended by removing the reference to \"No clause\" and replacing the words \"principal agent\" with \"employer\""]
[]
[null,"Clause 36.0 is amended by the addition of the following clause:"]
[]
[null,"36.7 Notwithstanding any clause to the contrary, on cancellation of this agreement either by the employer or the contractor; or for any reason whatsoever, the contractor shall on written instruction, discontinue with the works on a date stated and withdraw himself from the site. The contractor shall not be entitled to refuse to withdraw from the works on the grounds of any lien or right of retention or on the grounds of any other right whatsoever  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"A37.0 CANCELLATION BY EMPLOYER - LOSS AND DAMAGE  Clause 37.0  Clause 37.3.5 is amended by replacing \"ninety (90)\" with \"one hundred and twenty (120)\""]
[]
[null,"Clause 37.0 is amended by the addition of the following clause:  37.5 Notwithstanding any clause to the contrary, on cancellation of this agreement either by the employer or the contractor; or for any reason whatsoever, the contractor shall on written instruction, discontinue with the works on a date stated and withdraw himself from the site. The contractor shall not be entitled to refuse to withdraw from the works on the grounds of any lien or right of retention or on the grounds of any other right whatsoever  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"A38.0 CANCELLATION BY CONTRACTOR - EMPLOYER'S DEFAULT  Clause 38.0  Clause 38.5.4 is amended by replacing \"ninety (90)\" with \"one hundred and twenty (120)\"  Clause 38.0 is amended by the addition of the following clause:"]
[]
[null,"38.7 Notwithstanding any clause to the contrary, on cancellation of this agreement either by the employer or the contractor; or for any reason whatsoever, the contractor shall on written instruction, discontinue with the works on a date stated and withdraw himself from the site. The contractor shall not be entitled to refuse to withdraw from the works on the grounds of any lien or right of retention or on the grounds of any other right whatsoever  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"A39.0 CANCELLATION - CESSATION OF THE WORKS  Clause 39.0  Clause 39.3.5 is amended by the addition of the following at the end of the sentence:  \"within one hundred and twenty (120) working days of completion of such a report\"  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"DISPUTE"]
[]
[null,"A40.0 DISPUTE SETTLEMENT Clause 40.0  Clause 40.2.2 is amended by replacing \"one (1) year\" with \"three (3) years\"  Clause 40.6 is amended by removing the reference to:  No clause Clause 40.7.1 is amended by replacing \"(10)\" with \"(15)\" and by the addition of the following: Whether or not mediation resolves the dispute, the parties shall bear their own costs concerning the mediation and equally share the costs of the mediator and related costs "]
[]
[null,"SUBSTITUTE PROVISIONS"]
[]
[null,"A41.0 STATE CLAUSES  Clause 41.0  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"CONTRACT VARIABLES"]
[]
[null,"A42.0 THE SCHEDULE (DPW-04EC)  Clause 42.0  Tenderers are referred to the Contract Data DPW-04(EC) for variables pertaining to this contract  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"SECTION B: JBCC PRELIMINARIES"]
[]
[null,"B1.0 DEFINITIONS AND INTERPRETATION"]
[]
[null,"B1.1 Definitions and interpretation  See also clause A1.0 of Section A for additional and/or amended definitions which shall apply equally to this Section  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B2.0 DOCUMENTS"]
[]
[null,"B2.1 Checking of documents  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B2.2 Provisional bills of quantities  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B2.3 Availability of construction documentation  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B2.4 Interests of agents  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B2.5 Priced documents  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B2.6 Tender submission  Clause 2.6 is amended by replacing \"JBCC Form of Tender\" with \"Form of Offer and Acceptance DPW-07(EC)\"  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B3.0 THE SITE"]
[]
[null,"B3.1 Defined works area  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B3.2 Geotechnical investigation  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B3.3 Inspection of the site  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B3.4 Existing premises occupied  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B3.5 Previous work - dimensional accuracy  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B3.6 Previous work - defects  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B3.7 Services - known  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B3.8 Services - unknown  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B3.9 Protection of trees  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B3.10 Articles of value  Fixed:____________ Value related:____________ Time related:___________","Item",1]
[]
[null,"B3.11 Inspection of adjoining properties  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B4.0 MANAGEMENT OF CONTRACT"]
[]
[null,"B4.1 Management of the works  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B4.2 Programme for the works  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B4.3 Progress meetings  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B4.4 Technical meetings  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B4.5 Labour and plant records  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B5.0 SAMPLES, SHOP DRAWINGS AND MANUFACTURERS’ INSTRUCTIONS"]
[]
[null,"B5.1 Samples of materials  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B5.2 Workmanship samples  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B5.3 Shop drawings  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B5.4 Compliance with manufacturers' instructions  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B6.0 TEMPORARY WORKS AND PLANT"]
[]
[null,"B6.1 Deposits and fees  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B6.2 Enclosure of the works  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B6.3 Advertising  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B6.4 Plant, equipment, sheds and offices  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B6.5 Main notice board  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B6.6 Subcontractors' notice board  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B7.0 TEMPORARY SERVICES"]
[]
[null,"B7.1 Location  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B7.2 Water  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B7.3 Electricity  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B7.4 Telecommunication facilities  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B7.5 Ablution facilities  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B8.0 PRIME COST AMOUNTS"]
[]
[null,"B8.1 Responsibility for prime cost amounts  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B9.0 ATTENDANCE ON N/S SUBCONTRACTORS"]
[]
[null,"B9.1 General attendance  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B9.2 Special attendance  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B9.3 Commissioning - fuel, water and electricity  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B10.0 FINANCIAL ASPECTS"]
[]
[null,"B10.1 Statutory taxes, duties and levies  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B10.2 Payment for preliminaries  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B10.3 Adjustment of preliminaries Clauses B10.3.1 and B10.3.2 are amended by replacing \"within fifteen (15) working days of taking possession of the site\" with \"when submitting his priced bills of quantities / lump sum document\" Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B10.4 Payment certificate cash flow  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B11.0 GENERAL"]
[]
[null,"B11.1 Protection of the works  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B11.2 Protection / isolation of existing / sectionally occupied works  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B11.3 Security of the works  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B11.4 Notice before covering work  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B11.5 Disturbance  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B11.6 Environmental disturbance  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B11.7 Works cleaning and clearing  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B11.8 Vermin  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B11.9 Overhand work  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B11.10 Instruction manuals and guarantees  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B11.11 As built information  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B11.12 Tenant installations  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"B12.0 SCHEDULE OF VARIABLES"]
[]
[null,"B12.1 Schedule of variables  Fixed:____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"This schedule contains all variables referred to in this document and is divided into pre-tender and post-tender categories. The pre-tender category must be completed in full and included in the tender documents. Both the pre-tender and post-tender categories form part of these Preliminaries"]
[]
[null,"Spaces requiring information must be filled in, shown as \"not applicable\" or deleted and not left blank. Where choices are offered, the non-applicable items are to be deleted. Where insufficient space is provided the information should be annexed hereto and cross-referenced to the applicable clause of the schedule. Key cross reference clauses are italicised in [ ] brackets"]
[]
[null," 12.1 PRE-TENDER INFORMATION  12.1.1 Provisional bills of quantities [2.2] The quantities are provisional"]
[]
[null,"12.1.2 Availability of construction documentation [2.3] Construction documentation is complete"]
[]
[null,"12.1.3 Interests of agents [2.4] Details: "]
[]
[null,"12.1.4 Defined works area [3.1] Details: "]
[]
[null,"12.1.5 Geotechnical investigation [3.2] Details: "]
[]
[null,"12.1.6 Existing premises occupied [3.4] Specific requirements: "]
[]
[null,"12.1.7 Previous work - dimensional accuracy [3.5] Details: "]
[]
[null,"12.1.8 Previous work - defects [3.6]Details: "]
[]
[null,"12.1.9 Services - known [3.7] Details: "]
[]
[null,"12.1.10 Protection of trees [3.9] Specific requirements: "]
[]
[null,"12.1.11 Inspection of adjoining properties [3.11] Specific requirements: "]
[]
[null,"12.1.12 Enclosure of the works [6.2] Specific requirements: "]
[]
[null,"12.1.13 Offices [6.4.3] Specific requirements:  The contractor shall provide, maintain and remove on completion of the works an office for the exclusive use of the principal agent, minimum size 4 x 3 x 3m high internally, suitably insulated and ventilated, provided with electric lighting and fitted with boarded floor, desk, chair, drawing stool, drawing board and lock-up drawers for drawings. The office shall be kept clean and fit for use at all times"]
[]
[null,"12.1.14 Main notice board [6.5] Specific requirements:  The contractor shall provide, erect where directed, maintain and remove on completion of the works a notice board size 3 x 3m as type Drawing GEN 063, constructed of suitable boarding with flat smooth surface and with edging bead 19mm thick round outer edges and projecting 12mm from face of boarding and rounded on front edge. The board shall be securely fixed to hoarding, where hoarding is provided, or fixed to and including a suitable supporting structure of timber or tubular posts and braces. The board is to be painted ivory white and the bead and 12mm wide dividing lines dark green. All wording shall be inscribed in dark green as per the coat of arms for SA. All wording shall be inscribed in dark green painted sans serif lettering"]
[]
[null,"12.1.15 Subcontractors' notice board [6.6] A notice board is required"]
[]
[null," 12.1.16 Water [7.2] Option A (by contractor) YES/NO   Option C (by employer - metered)  YES/NO"]
[]
[null,"12.1.17 Electricity [7.3] Option A (by contractor)  YES/NO  Option C (by employer - metered) YES/NO"]
[]
[null,"12.1.18 Telecommunications [7.4] Telephone YES/NO   Facsimile    YES/NO    E-mail         YES/NO"]
[]
[null,"12.1.19 Ablution facilities [7.5] Option A (by contractor) YES/NO"]
[]
[null,"12.1.20 Protection of existing/sectionally occupied works [11.2] Protection is required"]
[]
[null,"12.1.21 Special attendance [9.2] Subcontractor (1) details:    Subcontractor (2) details:   Subcontractor (3) details:   "]
[]
[null,"12.1.22 Protection of the works [11.1] Specific requirements: "]
[]
[null,"12.1.23 Disturbance [11.5] Specific requirements: The contractor shall keep the site, structures, etc well watered during operations to prevent dust and shall provide and erect and remove on completion of the works all necessary temporary dust screens all to the satisfaction of the principal agent"]
[]
[null,"12.1.24 Environmental disturbance [11.6] Specific requirements: "]
[]
[null,"12.2 POST-TENDER INFORMATION"]
[]
[null,"12.2.1 Payment of preliminaries [10.2] Option A (prorated) Option B (calculated) YES/NO"]
[]
[null,"12.2.2 Adjustment of preliminaries [10.3] Option A (three categories) YES/NO"]
[]
[null,"12.2.3 Additional agreed preliminaries items  Details: "]
[]
[null,"SECTION C: SPECIFIC PRELIMINARIES"]
[]
[null,"Section C contains specific preliminary items which apply to this contract except where N/A (Not Applicable) appears against an item"]
[]
[null,"C1.0 CONTRACT DRAWINGS* Select relevant paragraph and delete whichever is not applicable depending on whether the contract is based on a bills of quantities or lump sum document* The drawings issued with the tender documents do not comprise the complete set but serve as a guide only for tendering purposes and for indicating the scope of the work to enable the tenderer to acquaint himself with the nature and extent of the works and the manner in which they are to be executed* A full set of drawings is issued with the tender documents indicating the full scope of the work to enable the tenderer to acquaint himself with the nature and extent of the works and the manner in which they are to be executed Should any part of the drawings not be clearly understood by the tenderer he shall, before submitting his tender, obtain clarification in writing from the principal agent Fixed: ____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"C2.0 GENERAL PREAMBLES  The document \"Specification of Materials and Methods to be used (PW371)\" is obtainable on the Department's website (http://www.publicworks.gov.za/ under \"Consultants Guidelines\"), and shall be read in conjunction with the bills of quantities / lump sum document and be referred to for the full descriptions of work to be done and materials to be used  Fixed: ____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"C3.0 TRADE NAMES Wherever a trade name for any product has been described in the bills of quantities / lump sum document, the tenderer's attention is drawn to the fact that any other product of equal quality may be used subject to the written approval of the principal agent being obtained prior to the closing date for submission of tenders If prior written approval for an alternative product is not obtained, the product described shall be deemed to have been tendered for Fixed: ____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"C4.0 IMPORTED MATERIALS AND EQUIPMENT  Where imported items are listed in the tender documents, the tenderer shall provide all the information called for, failing which the price of any such item, materials or equipment shall be excluded from currency fluctuations. (refer to Schedule of Imported Materials and Equipment DPW-23(EC) to be completed by tenderer)  Notwithstanding any provisions elsewhere regarding the adjustment of contract prices, the price of any item, material or equipment listed in terms of this clause shall be excluded from the Contract Price Adjustment Provisions (if applicable)  Fixed: ____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"C5.0 VIEWING THE SITE IN SECURITY AREAS  The site is situated in a security area and the tenderer must arrange with the unit commander or other responsible officer to obtain permission to enter the site for tendering purposes  Fixed: ____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"C6.0 COMMENCEMENT OF WORKS IN SECURITY AREAS  As the works falls within a security area the contractor must give the unit commander or other responsible officer notice before commencement of the works. Should the contractor fail to make such arrangements, admission to the site may be refused and any additional costs will be for the contractor's account  Fixed: ____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"C7.0 ENTRANCE PERMITS TO SECURITY AREAS  As the works falls within a security area the contractor shall obtain entrance permits for his personnel and workmen entering the area and shall comply with all regulations and instructions which may be issued from time to time regarding the protection of persons and property under the control of the Defence Force, Police or chief security officer  Fixed: ____________ Value related:____________ Time related:____________","Item",1]
[]
[null,"C8.0 SECURITY CHECK OF PERSONNEL  The principal agent may require the contractor to have his personnel and workmen, or a certain number of them, security classified  In the event of the principal agent requesting the removal of a person or persons from the works for security reasons, the contractor shall do so forthwith and shall thereafter ensure that such person or persons are denied access to the works and the site and/or to any document or information relating to the works  Fixed:____________ Value related:_____________ Time related:____________","Item",1]
[]
[null,"C9.0 PROHIBITION ON TAKING OF PHOTOGRAPHS  In terms of article 119 of the Defence Act, 44 of 1957, it is prohibited to sketch or to take photographs of any military site or installation or any building or civil works thereon or to be in possession of a camera or other apparatus used for taking of photographs except when authorized thereto by or on behalf of the Minister  The same prohibition is also applicable to all correctional institutions in terms of article 44.1(e) of the Correctional Services Act 8 of 1959  Fixed:_____________ Value related:____________ Time related:______________","Item",1]
[]
[null,"C10.0 HIV/AIDS AWARENESS  It is required of the contractor to thoroughly study the HIV/AIDS Specification (PW 1544) of the Department that must be read together with and is deemed to be incorporated under this Section of the bills of quantities / lump sum document. Provision for pricing of HIV/AIDS awareness is made under items C10.1 to C10.5 hereafter and it is explicitly pointed out that all requirements of the aforementioned specification are deemed to be priced hereunder, as the said items represent the only method of measurement and no additional items or extras to the contract in this regard shall be entertained  The contractor must take note that compliance with the HIV/AIDS Specification is compulsory. In the event of partial or total non-compliance, the principal agent, notwithstanding the provisions of clause A 31.0 of Section A or any other clause to the contrary, reserves the right to delay issuing any progress payment certificate until the contractor provides satisfactory proof of compliance. The contractor shall not be entitled to any compensation of whatsoever nature, including interest, due to such delay of payment"]
[]
[null,"C10.1 AWARENESS CHAMPION  Selection, appointment, briefing and making available of an Awareness Champion including provision of all relevant services, all in accordance with the HIV/AIDS Specification  Fixed:_____________ Value related:____________ Time related:______________","Item",1]
[]
[null,"C10.2 AWARENESS WORKSHOPS  Selection and appointment of a competent Service Provider approved by the principal agent, provision of a Service Provider Workshop Plan and a suitable venue, conducting of awareness workshops by means of traditional and/or modern multi-media techniques, including follow-up courses, making available all tuition material and performing assessment procedures, all in accordance with the HIV/AIDS Specification  Fixed:_____________ Value related:____________ Time related:______________","Item",1]
[]
[null,"C10.3 POSTERS, BOOKLETS, VIDEOS, ETC.  Provision, displaying, maintaining and replacing when necessary of four plastic laminated posters, booklets and educational videos, etc. for the duration of the construction period, all in accordance with the HIV/AIDS Specification  Fixed:_____________ Value related:____________ Time related:______________","Item",1]
[]
[null,"C10.4 ACCESS TO CONDOMS  Provision and maintenance of condom dispensers fixed in position, including male and female condoms, replenishing male and female condoms on a daily basis as required for the duration of the construction period, all in accordance with the HIV/AIDS Specification  Fixed:_____________ Value related:____________ Time related:______________","Item",1]
[]
[null,"C10.5 MONITORING  Monitoring HIV/AIDS awareness of workers, providing the principal agent with access to information including making available all reports, thoroughly completed and reflecting the correct information, for the duration of the construction period and close out, all in accordance with the HIV/AIDS Specification  Fixed:_____________ Value related:____________ Time related:______________","Item",1]
[]
[null,"C11.0 OCCUPATIONAL HEALTH AND SAFETY ACT  The contractor shall comply with all the requirements set out in the Construction Regulations, 2003 issued under the Occupational Health and Safety Act, 1993 (Act No 85 of 1993)  It is required of the contractor to thoroughly study the Health and Safety Specification that must be read together with and is deemed to be incorporated under this Section of the bills of quantities / lump sum document  The contractor must take note that compliance with the Occupational Health and Safety Act, Construction Regulations and Health and Safety Specification is compulsory.  In the event of partial or total non-compliance, the principal agent, notwithstanding the provisions of clause A31.0 of Section A or any other clause to the contrary, reserves the right to delay issuing any progress payment certificate until the contractor provides satisfactory proof of compliance.  The contractor shall not be entitled to any compensation of whatsoever nature, including interest, due to such delay of payment  Provision for pricing of the Occupational Health and Safety Act, Construction Regulations and Health and Safety Specification is made under this clause and it is explicitly pointed out that all requirements of the aforementioned are deemed to be priced hereunder and no additional claims in this regard shall be entertained  Fixed:_____________ Value related:____________ Time related:______________","Item",1]
[]
[null,"C11.1 NOTIFICATION OF CONSTRUCTION WORK (Construction Regulation 3) The Contractor shall, before commencing work, notify the Department of Labour of the intended construction work in terms of Regulation 3.  The Contractor shall submit the notification in writing, on the appropriate form, prior to commencement of work Fixed:_____________ Value related:____________ Time related:______________","Item",1]
[]
[null,"C11.2 HEALTH AND SAFETY PLAN (Construction Regulation 5.4) The Contractor shall provide and demonstrate to the Principal Agent a suitable and sufficiently documented health and safety plan based on the Act, Construction Regulations and the health and safety specification, which shall be applied from the date of commencement of and for the duration of the construction work.  The Contractor shall ensure that a copy of the health and safety plan is available on request to an employee, inspector, sub contractor or principal agent all in terms of Regulation 5Fixed:_____________ Value related:____________ Time related:______________","Item",1]
[]
[null,"C11.3 REGISTRATION WITH THE COMPENSATION FUND (Construction Regulation 5.3 f) The Contractor shall provide proof of his registration and good standing with the Compensation Fund or a licensed compensation insurer prior to the commencement of work Fixed:_____________ Value related:____________ Time related:______________","Item",1]
[]
[null,"C11.4 HEALTH AND SAFETY FILE ( Construction Regulation 5.7)  The Contractor shall ensure that a health and safety file, which shall include all documentation required in terms of the health and safety specification, the Act and the Construction Regulations, is opened and kept on site and made available to the Principal Agent or Inspector upon request.  Upon completion of the works, the Contractor shall hand over a consolidated health and safety file to the principal agent Fixed:_____________ Value related:____________ Time related:______________","Item",1]
[]
[null,"C11.5 SUPERVISION OF CONSTRUCTION WORK (SAFETY OFFICER) (Construction Regulation 6)  The Contractor shall appoint a full-time competent employee in writing as the construction supervisor, with the duty of supervising the construction work. The Contractor shall appoint a full-time or part-time construction safety officer in writing to assist in the control of all safety related aspects on the site. Such appointments are required to ensure that at all times the requirements of the Act and Construction Regulations are adhered to. Refer to Regulation 6  Fixed:_____________ Value related:____________ Time related:______________","Item",1]
[]
[null,"C11.6 RISK ASSESSMENT AND SAFETY POLICY (Construction Regulation 7)  Before commencing work the Contractor shall cause a risk assessment to be performed by a competent person appointed in writing and the risk assessment shall form part of the health and safety plan. A copy of the risk assessment shall be available on site at all times for inspection. The Contractor shall at all time carry out the works in a manner to avoid the risk of bodily harm to persons or risk of damage to any property.  He shall take all precautions regarding training of employees in any hazards and the related work procedures, health and safety induction training of employees, visitors or any other persons entering the site and provide personal protective equipment to all employees and visitors to site which are necessary and adequate to eliminate any conditions which contribute to the risk of injury to persons or damage to property in terms of Regulation 7  Fixed:_____________ Value related:____________ Time related:______________","Item",1]
[]
[null,"C11.7 SIGNIFICANT HAZARDA IDENTIFICATION RISK ASSESSMENT PREPARED BY THE DESIGN CONSULTANTS  The contractor shall allow for additional financial provision, if any, to take the necessary precautions regarding the significant hazards and risks identified and assessed by the design consultants  Fixed:_____________ Value related:____________ Time related:______________","Item",1]
[]
[null,"C11.8 ADDITIONAL FINANCIAL PROVISION  The Contractor shall allow for additional financial provision, if any, to comply with the requirements of the Occupational Health and Safety Act  (Act No 85 of 1993) and the Construction Regulations issued there under which have not been specifically elsewhere provided  Fixed:_____________ Value related:____________ Time related:______________","Item",1]
[]
[null,"C11.9 FALL PROTECTION PLAN (Construction Regulation 8)  The contractor shall, before commencing any construction work submit a fall protection plan identified all steps to be taken in order to ensure the continued adherence to the fall protection plan and shall include a risk assessment of all work carried out from an relevant position. The fall protection plan shall form part of the health and safety plan and file  Fixed:_____________ Value related:____________ Time related:______________","Item",1]
[]
[null,"C11.10 PHYSICAL AND PSYCHOLOGICAL FITNESS (Construction Regulation 8.2(b))  The contractor and sub-contractors shall before commencing any construction work submit proof of his employees that shall carried out work from an elevated position their physical and psychological fitness. And shall be recorded in the health and safety file  Fixed:_____________ Value related:____________ Time related:______________","Item",1]
[]
[null,"C11.11 CONSTRUCTION VEHICLES AND MOBILE PLANT (Construction Regulation 21)  The contractor and sub-contractors shall ensure that all operated workers received training and been certified competent to operate such vehicle, and are physical and psychological fit to operate such construction vehicles and mobile plants. And shall be recorded in the health and safety file  Fixed:_____________ Value related:____________ Time related:______________","Item",1]
[]
[null,"C11.12 TRAINING (Construction Regulation 8 (c))  The contractor and sub-contractors shall, before commencing any construction work, submit his training program of all his employees. This program shall from part of the health and safety plan  Fixed:_____________ Value related:____________ Time related:______________","Item",1]
[]
[null,"C11.13 DEMOLITION WORK (Construction Regulation 12)  The contractor shall, before any demolition work shall carried out, submit all method of demolition to be used. This method shall form part of the health and safety plan and file.  Fixed:_____________ Value related:____________ Time related:______________","Item",1]
[]
[null,"C11.14 REMOVAL AND DISPOSAL OF ASBESTOS MATERIAL (Asbestos Regulation) The principle contractor shall appoint a contractor that is registered with the Department of Labour as an AIA. The contractor must allow for; NOTIFICATION OF ASBESTOS PROCESSINGPERSONAL PROTECTIVE EQUIPMENTPACKAGING AND TRANSPORT AND STORAGE TO DISPOSAL SITEDEMOLITION WORK OF SHEETSLABELLING AND INFORMATIONFixed:_____________ Value related:____________ Time related:______________","Item",1]
[]
[]
[]
[null,"Carried to Summary"]
[]
[null,"SECTION NO.2"]
[null,"BLOCK A - GUARD HOUSE"]
[null,"BILL NO.1"]
[null,"ALTERATIONS AND DEMOLITIONS"]
[]
[null,"PREAMBLES"]
[null,"The  tenderer  is  referred  to  the  relevant  clauses  in  the separate  document  Model  Preambles  for  Trades  (2017 Edition) and to the Supplementary Preambles which are incorporated in this Bill."]
[]
[null,"Damage and Repairs to Services\nShould the Contractor damage  any services which  are to  remain  in  operation  or  any  services  which  have  not yet   been   disconnected   prior   to   removal,   then   the Contractor   will   be   held   soley   responsible   for   such damage and any further resultant damage.\nThe     Contractor     shall     immediately     notify     the Representative/Agent   and   the   Authorities   concerned and   he   shall   at   his   own   cost   make   all   necessary arrangements  for  disconnection  and  repairs  with  the relevant  Authorities  and  shall pay  all  fees  and  charges levied.\nDisposal of Materials\nAll   existing   materials   specified   to    be   \"removed\", demolished   and   removed\",   \"hacked   up   or   off   and removed\",   or   \"taken   down   or   off   and  removed\"   or \"broken down and removed\", etc., become the property of the contractor. These materials and all debris, rubbish and  earth  must  be  carted  away  by  the  Contractor  and the  site  must  be  left  clean  and  unencumbered.  The Contractor   must   make   his   own   arrangements   for\ndumping and shall pay all fees and charges levied."]
[]
[null,"If  any  of  the  bricks  or  other  materials  specified  to  be \"removed\"  are  sound  and  considered  suitable  for  any portion   of   the   new   work   they   must   be   thoroughly cleaned  off  and  stacked  on  site  for  inspection  by  the Representative/Agent must be obtained before any such materials are re-used in the new work.\nAll  existing  materials  specified  to  be  \"taken  down  and set aside for re-use\" or \"taken down and set aside\" shall remain  the  property  of  Employer  and  must  be  cleaned off,  cleared  off  all  nails,  etc.  and  neatly  stacked  and stored  on  site  by  the  Contractor  where  directed  and carefully  handled  during  taking  down,  storage  and  re- fixing.  The  Contractor  will  be  held  responsible  for  the safety  of  these  materials  and  must  take  all  necessary precautions for their protection and any damage or loss that may occur must be made good by the Contractor at his own expense.\nThe Contractor must visit the site and the buildings and acquaint   himself   fully   with   conditions   and   scope   of alterations and demolitions. Descriptions herein are brief and  are  to  serve  as  a  means  of  identifying  work  only. The   full   extent   of   work   is   to   be   assessed   by   the contractor on site. All sizes indicated are approximate.\nRates  for  demolitions  and  alterations  are  to  include  for all  needling,  strutting  and  shoring,  etc.  that  may  be necessary whilst carrying out any portion of the work to ensure  the  stability  of  the  building  with  suitable  and substantial    materials    to    the    satisfaction    of    the Representatitve/Agent and remove when directed.\nOld Materials to become the property of the contractor."]
[]
[null,"Old  materials from  alterations, except where  described to be  re-used  or  handed  over,  become  the property  of the   contractor   who   must   allow   credit   in   the   final summary.\nOld Materials to be carted away:"]
[]
[null,"Old  materials from  alterations, except where  described to  be  re-used  or  handed  over,  as  well  as  rubbish,  etc. must be regularly carted from site and not to be allowed\nto accumulate on or around the site."]
[]
[null,"Handling over of materials"]
[]
[null,"Where  certain  materials  or  articles  from  alterations  are described  to  be  handed  over  by  the  contractor  to  the Regional    Representative/Agent,    such    materials    or articles  shall  be  properly  stored  by  the  contractor,  until handling over thereof.\nThe Contractor must obtain an official receipt listing the materials  or  articles  and  dates  of  handing  over.  If  the contractor fails to submit the receipt when requested to do so,  it  shall be  deemed  that  the  materials  or  articles are  still  in  his  possession  and  he  will  be  held  liable  to the  Municipality  for  the  full  replacement  value  thereof, which  will  be  deducted  from  any  monies  due  to  the Contractor.\nTEMPORARY BARRIERS, SCREENS, ETC."]
[]
[null,"Temporary barriers, screens, etc. and including removal"]
[]
[null,"1     Provide,  fix,  maintain,  move  and  subsequently  remove all  temporary  barriers,  screens,  overhead  projections, etc.  that  may  be  necessary  whilsy  carrying  out  any portion of the work for the protection of persons, animals and things, including the protection of existing buildings, structures, pavings and services on the remainder of the\nsite"]
[]
[null,"REMOVAL OF EXISTING WORK"]
[null,"Taking down and removing roofs, floors, panelling, ceilings, partitions, etc"]
[]
[null,"RhinoBoard ceiling, including cornices, timber\nbrandering, etc.","m2",4]
[]
[null,"Taking    up    and    removing    wood     block    floor coverings,  vinyl  floor  coverings,  carpets,  etc  and preparing screeds for new floor coverings"]
[]
[null,"Vinyl tile floor covering","m2",4]
[]
[null,"Taking out and removing sundry joinery work"]
[]
[null,"Timber skirtings from brickwork","m",8]
[]
[null,"Taking out and removing doors, ironmongery"]
[]
[null,"Timber single door including iromongery","No",1]
[]
[null,"Take out steel door frame and prepare to fix new","No",1]
[]
[null,"Removal of timber roof structure composed of purlins, trusses wall plates, etc. complete and prepare to receive new roof structure"]
[]
[null,"Roof structure overall size 2254mm long x 1884mm wide x 1750mm high","No",1]
[]
[null,"PREPARATORY WORK TO EXISTING SURFACES"]
[null,"Sika repair system' or similar approved"]
[]
[null,"Repair concrete surface with SIKA monotop 615 on SIKA monotop primer, then seal with SIKAFLEX, as per manufacturer's specification","m2",4]
[]
[null,"MAKING GOOD OF FINISHES, ETC."]
[null,"Making good"]
[]
[null,"Make good  affected  100mm  thick  surface  beds  and screed to floors (Guard House)","m2",4]
[]
[null,"SECTION NO.2 - BLOCK A - GUARD HOUSE"]
[]
[null,"CONCRETE, FORMWORK AND REINFORCEMENT"]
[]
[null,"PREAMBLES"]
[null,"The  tenderer  is  referred  to  the  relevant  clauses  in  the separate  document  Model  Preambles  for  Trades  (2017 Edition) and to the Supplementary Preambles which are incorporated in this Bill.\n_"]
[null,"Cost of tests\nThe cost of making, storing and testing of concrete test cubes as required under clause 7 'Test' of SABS1200G shall   include   the   cost   of   providing   cube   moulds necessary  for  the  purpose,  for  testing  costs  and  for submitting  reports  on  the  tests  to  the  Architect.  The testing  shall  be  undertaken  by  an  independent  firm  or institution nominated by the  Contractor to the  approval of the Architect. (Test cubes are measured separately).\nFormwork:\nDescriptions  of  formwork  shall  be  deemed  to  include use and waste only (except where described as left in or permanent),  for  fitting  together  in  the  required  forms, wedging,   plumbing   and   fixing   to   true   angles   and surfaces  as  necessary  to  ensure  easy  release  during stripping and for reconditioning as necessary before re- use.\n"]
[]
[null,"CONCRETE"]
[null,"25 Mpa /19mm concrete"]
[]
[null,"Apron","m3",1]
[]
[null,"TEST BLOCKS"]
[]
[null,"Making and   testing   150   x   150   x   150mm   concrete strength test cube (Provisional)","no",1]
[]
[null,"CONCRETE SUNDRIES"]
[null,"Finishing top surface of concrete smooth with a power float"]
[]
[null,"Surface beds,slabs, etc. (Provisional)","m2",10]
[]
[null,"FORMWORK"]
[null,"ROUGH FORMWORK (DEGREE OF ACCURACY II)"]
[]
[null,"Apron","m2",1]
[]
[null,"PREAMBLES"]
[null,"The  tenderer  is  referred  to  the  relevant  clauses  in  the separate document Model Preambles for Trades  (2017 Edition) and to the Supplementary Preambles which are incorporated in this Bill."]
[]
[null,"PROFILED METAL SHEETING AND"]
[null,"ACCESSORIES"]
[null,"Chromadek (10.5) corrugated 0,8mm thick ISOQ230 Dove Grey pre-painted with chromadek finish to one side  and  with protective  primer  coating  on  reverse side,  interlocking   galvanised   steel   roof   sheeting with  Z275  spelter  sheeting  to  both  sides  fixed  to timber  purlins  (elsewhere)  with  clips  screw,  all  in accordance  with  manufacturer's  recommendations and specifications"]
[]
[null,"Roof covering with pitches not exceeding 25 degrees with side laps seam stitched","m2",6]
[]
[null,"Ridge cappings 450mm girth","m",2]
[]
[null,"Standard narrow and broad flute closers","m",4]
[]
[null,"Moulded narrow and broad rib polyethylene filler blocks","m",4]
[]
[null,"ROOF AND WALL INSULATION"]
[null,"\"Sisalation 420\" heavy industrial grade aluminium foil based insulation"]
[]
[null,"Insulation   sheeting   laid   taut   over   purlins   and   fixed concurrent  with  roof  covering  with  minimum  150mm stapled   laps   including   steel   straining   wires   at   not exceeding 400mm centres and double sided tape at\nedges where required","m2",6]
[]
[null,"SECTION NO.2 - BLOCK A - GUARD HOUSE"]
[]
[null,"BILL NO.4 "]
[null,"CARPENTRY AND JOINERY"]
[]
[null,"PREAMBLES"]
[null,"The  tenderer  is  referred  to  the  relevant  clauses  in  the separate  document  Model  Preambles  for  Trades  (2017 Edition) and to the Supplementary Preambles which are incorporated in this Bill."]
[]
[null,"Fixing:\nItems  described  as  nailed  shall  be  deemed  to be  fixed with  hardened  stainless  steel  nails/slots  pins/spinless screws to brick or concrete.\nFixing brackets to be hot dipped galvanised where items not specifically mentioned.\nItems   described   as   \"plugged\"   shall   be   deemed   to include  screwing  to  fibre,  plastic  or  metal  plugs  at  not exceeding  500mm  centres,  and  where  described  as \"bolted\", the bolts have been given elsewhere\nDecorative thermosetting plastic laminate covering"]
[]
[null,"Laminate  covering  shall  be  glued  under  pressure  and edge  strips  of  same  shall  be  butt  jointed  at  junctions with adjacent similar finish"]
[]
[null,"ROOFS ETC"]
[null,"PLATE NAILED TIMBER ROOF TRUSS CONSTRUCTION, ETC.",{"$nulls":7},833347501]
[]
[null,"SUPPLEMENTARY PREAMBLES"]
[null,"Tenderers are to make allowance in their rates for additional expenses in regard to treatment of timber against insect pest affecting softwood fixed permanently in the building\nThe design of prefabricated roof trusses, bracings and secondary members forming part of the total timber roof construction shall be prepared by a professional structural engineer- Truss System Engineer\nA copy of letter reference TR1 and TR2 must be completed and signed by the Truss System Engineer and submitted to the Architect\nThe tenderer is to allow in his rates for the roof trusses for the design, manufacture, supply, hoisting and fixing of the roof trusses and permanent bracings, any necessary temporary bracing, and for the costs of all inspections by the Truss System Engineer\nRoof pitch is to be 17.5 degrees\nCeilings are 6.0mm Gypsum on 38 x 38mm brandering at 400 c/c\nThe dimensions in the description of the trusses are nominal and actual measurements are to be obtained from the Architect/Engineers and or taken on site before design or fabrication.\nSawn treated softwood grade V4"]
[]
[null,"1     Roof construction to double pitched roof 2554mm long x 2554mm wide x 1750mm high (17.5 degrees pitch) with 600mm overhang on both sides including trusses, runners, bracings etc (all plates, purlins hurricane clips,\nelsewhere measured) ","No",1]
[]
[null,"38 x 114mm Wall plates","m",9]
[]
[null,"50 x 76mm Purlins","m",20]
[]
[null,"Extra over for 300mm long wrought end to purlins","No",16]
[]
[null,"76 x 76mm Splayed purlins","m",6]
[]
[null,"Supply Performance certificate to certify that the roof has been constructed and erected in accordance with approved design (TR1 and TR2 Certificates)","item"]
[]
[null,"Two coats \"ABE provonite\" paint on exposed roof timbers and wall plates","m2",16]
[]
[null,"\"Teco\" two way hurricane clips","No",20]
[]
[null,"DOORS, ETC\nRefer to Architectural door schedule. \"Saligna Blaco\""]
[]
[null,"40mm  Framed  ledged  and  braced  batten  door  813  x 2032mm high with 40 x 110mm styles and top rail, 20 x 150mm middle ledge, 20 x 225mm bottom ledge and 20 x 110mm braces filled in with V-jointed one side vertical boarding with tongued and grooved joints to top rail and stiles and with inner edges of framing and abutting\nedges of boarding chamfered to form V-joint (D1) ","No",1]
[]
[null,"SKIRTINGS"]
[null,"Wrought meranti\n10     19   x   76mm   Skirtings  with   19mm   quadrant   bead,\nplugged.","m",8]
[]
[null,"Purpose made:\n11     Worktop  with  drawer  and  lockable  cupboard  as  per\nArchitectural drawing complete ","No",1]
[]
[null,"SECTION NO.2 - BLOCK A - GUARD HOUSE"]
[null,"CEILINGS, PARTITIONS AND ACCESS FLOORING"]
[null,"PREAMBLES"]
[null,"The  tenderer  is  referred  to  the  relevant  clauses  in  the separate  document  Model  Preambles  for  Trades  (2017 Edition) and to the Supplementary Preambles which are incorporated in this Bill."]
[]
[null,"Fixing\nItems described as \"nailed\" shall be deemed to be fixed with hardened steel nails  or pins, or to be shot-pinned, to brickwork or concrete\nItems   described   as   \"plugged\"   shall   be   deemed   to include  screwing  to  fibre,  plastic  or  metal  plugs  at  not exceeding  500mm  centres,  and  where  described  as \"bolted\", the bolts have been given elsewhere\nCeilings"]
[]
[null,"Unless otherwise described ceilings shall be deemed to be horizontal\nCEILINGS, ETC."]
[]
[null,"6.5mm Gypsum plasterboard with H-profile metal steel jointing strips"]
[]
[null,"Ceilings including 50 x 50mm sawn softwood brandering at  400mm  centres  generally  in  one  direction  and  50  x 50mm branders and cross branders at joints and edges of boards","m2",4]
[]
[null,"Extra  over  ceiling  for  600  x  600mm  trap  door  of  38  x 114mm   softwood   rebated   framing   with   one   cross brander,  covered  with  ceiling  board  and  fitted  flush  in opening, including necessary trimmers around","No",1]
[]
[null,"\"Rhino\" gypsum plasterboard cornices"]
[]
[null,"75mm Coved cornices","m",8]
[]
[null,"\"Isotherm\" insulation"]
[]
[null,"50mm   Insulation   closely  fitted   and   laid   on   top   of brandering between roof timbers, etc "]
[]
[null,"SECTION NO.2 - BLOCK A - GUARD HOUSE"]
[null,"BILL NO.6"]
[]
[null,"PREAMBLES"]
[null,"The  tenderer  is  referred  to  the  relevant  clauses  in  the separate  document  Model  Preambles  for  Trades  (2017 Edition) and to the Supplementary Preambles which are incorporated in this Bill."]
[]
[null,"SUPPLEMENTARY PREAMBLES"]
[]
[null,"Fixing"]
[null,"Floor coverings, wall linings, etc shall, where applicable, be   fixed   with   adhesive   as   recommended   by   the manufacturers of the flooring, linings, etc"]
[]
[null,"FLOOR COVERINGS"]
[null,"VINYL FLOOR COVERINGS"]
[null,"2mm thick x 1200mm wide Superflex fully flexible vinyl floor tiles"]
[null,"On floors","m2",4]
[]
[null,"POLISH, SEALERS, ETC"]
[null,"Three coats waterbased sealer on vinyl flooring.","m2",4]
[]
[null,"SECTION NO.2 - BLOCK A - GUARD HOUSE"]
[null,"BILL NO.7"]
[]
[null,"IRONMONGERY"]
[null,"PREAMBLES"]
[null,"The  tenderer  is  referred  to  the  relevant  clauses  in  the separate document Model Preambles for Trades  (2017 Edition) and to the Supplementary Preambles which are incorporated in this Bill."]
[]
[null,"LOCKS"]
[null,"\"Dorma\" or similar approved"]
[null,"\"Ref 390/313\" four-lever mortice lockset","No",1]
[]
[null,"SUNDRIES"]
[null,"38mm Diameter rubber door stop plugged","No",1]
[]
[null,"KEY TAGS"]
[null,"28mm  Diameter  x  1mm  thick  brass  key  tags  with  one numeral and one letter engraved","No",1]
[]
[null,"Approved standard stainless steel key rings","No",1]
[]
[null,"SECTION NO.2 - BLOCK A - GUARD HOUSE"]
[null,"BILL NO.8"]
[]
[null,"METALWORK"]
[null,"PREAMBLES"]
[null,"The  tenderer  is  referred  to  the  relevant  clauses  in  the separate  document  Model  Preambles  for  Trades  (2017 Edition) and to the Supplementary Preambles which are incorporated in this Bill."]
[null,"_"]
[null,"SUPPLEMENTARY PREAMBLES"]
[null,"Descriptions of bolts, anchors, etc"]
[null,"Descriptions of bolts shall be deemed to include nuts and washers"]
[null,"Descriptions   of   expansion   anchors   and   bolts   and chemical anchors and bolts shall be deemed to include nuts, washers and mortices in brickwork or concrete"]
[null,"Items described as \"holed for bolt(s)\" shall be deemed to exclude the bolts unless otherwise described"]
[null,"Items   described   as   \"plugged\"   shall   be   deemed   to include  screwing  to  fibre,  plastic  or  metal  plugs  at  not exceeding 600mm centres"]
[]
[null,"GALVANISED PRESSED STEEL DOOR FRAMES"]
[null,"1,2mm Thick double rebated door frames with 1 pair steel  butt  hinges,  chromium  plated  striking   plate and rubber buffers suitable for half brick walls"]
[null,"Frame for door 900 x 2032mm high","No",1]
[]
[null,"SECTION NO.2 - BLOCK A - GUARD HOUSE"]
[null,"BILL NO.9"]
[null,"GLAZING"]
[null,"PREAMBLES"]
[null,"The  tenderer  is  referred  to  the  relevant  clauses  in  the separate  document  Model  Preambles  for  Trades  (2017 Edition) and to the Supplementary Preambles which are incorporated in this Bill."]
[null,"_"]
[null,"(CPAP WORK GROUP NO. 150) unless\notherwise stated"]
[null,"GLAZING TO STEEL WITH PUTTY"]
[null,"6mm Clear float glass"]
[null,"Panes exceeding 0,1m2 and not exceeding 0,5m2","m2",7]
[]
[null,"SECTION NO.2 - BLOCK A - GUARD HOUSE"]
[null,"BILL NO.9"]
[null,"PAINTWORK"]
[null,"The  tenderer  is  referred  to  the  relevant  clauses  in  the separate  document  Model  Preambles  for  Trades  (2017 Edition) and to the Supplementary Preambles which are incorporated in this Bill."]
[]
[null,"PAINT SPECIFICATIONS\nAll painting shall be done in accordance with \"Plascon\" specifications unless otherwise described\nPrime  all  skirtings  and  timber  work  not  visible  prior  to installation. Further  paint  all  glazing  beads  and  reveals prior to glazing.\nPrimers  and  first  coats  may  be  thinned  in  accordance with the paint specifications to aid the absorption of the paint.\nWhere  surfaces  of  plaster  etc  are  sandy  /  friable,  the first  coat  must  be  replaced  with  'Merit'  plaster  primer thinned 10% with turpentine.\nAll surfaces must be sound, clean and have a moisture content  of less than 8% for walls generally and 3% for slabs/screeds etc.\nThe  paint  and  surface  finishes  specified  herein  are  for normal  applications  as  intended  by  the  manufacturer. Should a finish be required for a surface other than that\nfor  which  it  would  normally  be  used,  then  the  specifier should contact manufacturer for approval."]
[]
[null,"COLOURS"]
[null,"Unless   otherwise   described   all   paintwork   shall   be deemed  to  have  a  colour  value  in  excess  of  7  on  the Munsell system in accordance with SANS 1091"]
[]
[null,"PAINTWORK ETC."]
[null,"ON INTERNAL FLOATED PLASTER SURFACES"]
[]
[null,"Prepare  surfaces  and   remove  all  loose  material, apply  one  coat  'Plascon  Wall  and  All  Pure  Acrylic' thinned  20%  and  one  coat  'Plascon  Wall  and   All Pure Acrylic' paint or equal and approved:"]
[]
[null,"On internal walls","m2",22]
[]
[null,"External walls","m2",22]
[]
[null,"ON PLASTERBOARD"]
[null,"Prepare  surfaces  and   remove  all  loose  material, apply one coat 'Merit Plaster Primer' and two coats 'Plascon  Double Velvet  Pure  Acrylic'  paint  or equal and approved:"]
[null,"On ceilings and cornices.","m2",4]
[]
[null,"ON METAL"]
[null,"Prepare  surfaces  and  remove  all  loose   material, dust,   grease,   salts    and   contamination   with    a degreaser,   rinse   and   apply   one   coat   Calcium Plumbate Primer, one coat Universal Undercoat and two  coats  High  Gloss  Enamel  paint  on  galvanised steel:"]
[]
[null,"On door frame","m2",1]
[]
[null,"On gates  ","m2",3]
[]
[null,"ON WOOD"]
[null,"On doors","m2",3]
[]
[null,"ON FIBRE-CEMENT"]
[null,"Apply Plascon meit plaster primer and two coats Plascon Velvaglo Polyurethane Enamel paint."]
[null,"Fascias and barge boards.","m",6]
[]
[null,"SECTION SUMMARY - BLOCK A - GUARD HOUSE"]
[]
[null,"Alterations and Demolitions"]
[]
[null,"Concrete, Formwork and Reinforcement"]
[]
[null,"Roof Coverings"]
[]
[null,"Carpentry and Joinery"]
[]
[null,"Ceilings, Partitioning and Access Flooring"]
[]
[null,"Floor Coverings"]
[]
[null,"Ironmongery"]
[]
[null,"Metalwork"]
[]
[null,"Glazing"]
[]
[null,"Paintwork"]
[]
[null,"SECTION NO.3 BLOCK B, C AND D - ABLUTION BLOCKS"]
[]
[null,"BILL NO.1 ALTERATIONS AND DEMOLITIONS"]
[null,"PREAMBLES"]
[null,"The  tenderer  is  referred  to  the  relevant  clauses  in  the separate  document  Model  Preambles  for  Trades  (2017 Edition) and to the Supplementary Preambles which are incorporated in this Bill.\n_\nSUPPLEMENTARY PREAMBLES"]
[null,"Damage and Repairs to Services\nShould the Contractor damage  any services which  are to  remain  in  operation  or  any  services  which  have  not yet   been   disconnected   prior   to   removal,   then   the Contractor   will   be   held   soley   responsible   for   such damage and any further resultant damage.\nThe     Contractor     shall     immediately     notify     the Representative/Agent   and   the   Authorities   concerned and   he   shall   at   his   own   cost   make   all   necessary arrangements  for  disconnection  and  repairs  with  the relevant  Authorities  and  shall pay  all  fees  and  charges levied.\nDisposal of Materials\nAll   existing   materials   specified   to    be   \"removed\", demolished   and   removed\",   \"hacked   up   or   off   and removed\",   or   \"taken   down   or   off   and  removed\"   or \"broken down and removed\", etc., become the property of the contractor. These materials and all debris, rubbish and  earth  must  be  carted  away  by  the  Contractor  and the  site  must  be  left  clean  and  unencumbered.  The Contractor   must   make   his   own   arrangements   for\ndumping and shall pay all fees and charges levied."]
[]
[null,"If  any  of  the  bricks  or  other  materials  specified  to  be \"removed\"  are  sound  and  considered  suitable  for  any portion   of   the   new   work   they   must   be   thoroughly cleaned  off  and  stacked  on  site  for  inspection  by  the Representative/Agent must be obtained before any such materials are re-used in the new work.\nAll  existing  materials  specified  to  be  \"taken  down  and set aside for re-use\" or \"taken down and set aside\" shall remain  the  property  of  Employer  and  must  be  cleaned off,  cleared  off  all  nails,  etc.  and  neatly  stacked  and stored  on  site  by  the  Contractor  where  directed  and carefully  handled  during taking down,  sotorage and re- fixing.  The  Contractor  will  be  held  responsible  for  the safety  of  these  materials  and  must  take  all  necessary precautions for their protection and any damage or loss that may occur must be made good by the Contractor at his own expense.\nThe Contractor must visit the site and the buildings and aquaint   himself   fully   with   conditions   and   scope   of alterations and demolitions. Descriptions herein are brief and  are  to  serve  as  a  means  of  identifying  work  only. The   full   extent   of   work   is   to   be   assessed   by   the contractor on site. All sizes indicated are approximate.\nRates  for  demolitions  and  alterations  are  to  include  for all  needling,  strutting  and  shoring,  etc.  that  may  be necessary whilst carrying out any portion of the work to ensure  the  stability  of  the  building  with  suitable  and substantial    materials    to    the    satisfaction    of    the Representatitve/Agent and remove when directed.\nOld Materials to become the property of the contractor."]
[]
[null,"Old  materials from  alterations, except where  described to be  re-used  or  handed  over,  become  the property  of the   contractor   who   must   allow   credit   in   the   final summary.\nOld Materials to be carted away:"]
[]
[null,"Old  materials from  alterations, except where  described to  be  re-used  or  handed  over,  as  well  as  rubbish,  etc. must be regularly carted from site and not to be allowed\nto accumulate on or around the site."]
[]
[null,"Where  certain  materials  or  articles  from  alterations  are described  to  be  handed  over  by  the  contractor  to  the Regional    Representative/Agent,    such    materials    or articles  shall  be  properly  stored  by  the  contractor,  until handling over thereof.\nThe Contractor must obtain an official receipt listing the materials  or  articles  and  dates  of  handing  over.  If  the contractor fails to submit the receipt when requested to do so,  it  shall be  deemed  that  the  materials  or  articles are  still  in  his  possession  and  he  will  be  held  liable  to the  Municipality  for  the  full  replacement  value  thereof, which  will  be  deducted  from  any  monies  due  to  the Contractor.\n"]
[null,"TEMPORARY BARRIERS, SCREENS, ETC.\nTemporary barriers, screens, etc. and including removal","item",1]
[null,"Provide,  fix,  maintain,  move  and  subsequently  remove all  temporary  barriers,  screens,  overhead  projections, etc.  that  may  be  necessary  whilst  carrying  out  any portion of the work for the protection of persons, animals and things, including the protection of existing buildings, structures, pavings and services on the remainder of the site","item",1]
[]
[null,"REMOVAL OF EXISTING WORK"]
[null,"Taking out and removing doors, ironmongery","No",26]
[]
[null,"Take out and remove wall tiles"]
[null,"Existing wall tile","m2",16]
[]
[null,"BUDGETARY ALLOWANCE"]
[null,"Allow   the   budgetary   amount   of   R   50    000    (Fifty Thousand   Rands)   to   be   used   for   any   unforeseen alterations or omitted in part or in whole as required for additional builder's work not to be used at the discretion of contractor.",null,1,50000]
[]
[null,"SECTION NO.3 BLOCK B, C AND D - ABLUTION BLOCKS"]
[]
[null,"BILL NO.2 ROOF COVERINGS, ETC."]
[null,"PREAMBLES"]
[null,"The  tenderer  is  referred  to  the  relevant  clauses  in  the separate document Model Preambles for Trades  (2017 Edition) and to the Supplementary Preambles which are incorporated in this Bill"]
[]
[null,"SERVICE, REPAIRS, ETC. TO EXISTING"]
[null,"WORKS"]
[null,"Service, repair and make good existing roof coverings Service  and  make  good  the  existing  roof  coverings including   refixing   roof   sheets   with   new   galvanised screws, patching all roof leaks with derbigum and leave roof  in  fully  functional  state  for  end  user.  (Provisional)\n(All leaking roofs iBlocks B, C and D)","M2",102]
[]
[null,"SECTION NO.3 BLOCK B, C AND D - ABLUTION BLOCKS"]
[]
[null,"CARPENTRY AND JOINERY"]
[null,"PREAMBLES"]
[null,"The  tenderer  is  referred  to  the  relevant  clauses  in  the separate document Model  Preambles for Trades  (2017 Edition) and to the Supplementary Preambles which are incorporated in this Bill."]
[]
[null,"SUPPLEMENTARY PREAMBLES"]
[null,"Fixing:"]
[null,"Items described as nailed shall  be deemed to be  fixed with hardened  stainless  steel  nails/slots  pins/spinless screws to brick or concrete. Fixing brackets to be hot dipped galvanised where items not specifically mentioned. Items  described   as   \"plugged\"   shall   be   deemed   to include  screwing  to  fibre,  plastic  or  metal  plugs  at  not exceeding 500mm  centres,  and  where  described  as \"bolted\", the bolts have been given elsewhere Decorative thermosetting plastic laminate covering Laminate  covering  shall  be  glued  under  pressure  and edge  strips  of  same  shall  be  butt  jointed  at  junctions with adjacent similar finish"]
[]
[null,"ROOF STRUCTURE"]
[null,"Allow for roof structure repairs for damaged and  rotten roof timber members for roof overall size 1900  x 9760mm long (Block D) ","item"]
[]
[null,"Allow for roof structure repairs for damaged and  rotten roof timber members for roof overall size 1940  x 6059mm long (Block C)","item"]
[]
[null,"Allow  for  roof  structure  repairs  for  damaged and rotten roof   timber   members   for   roof   overall  size   13820   x 5150mm long (Block B)","item"]
[]
[null,"DOORS, ETC.\nRefer to Architectural door schedule.\n"]
[null,"Semisolid  flush  core  timber  door  with  masonite veneer hung to 1.2mm galvanised steel door frames (elsewhere)"]
[null,"44mm x 730 x 2032mm high single door with 100mm undercut ","No",24]
[]
[null,"SOLID DOORS"]
[null,"\"Saligna Blaco\""]
[null,"40mm  Framed  ledged  and  braced  batten  door  813  x 2032mm high with 40 x 110mm styles and top rail, 20 x 150mm middle ledge, 20 x 225mm bottom ledge and 20 x 110mm braces filled in with V-jointed one side vertical boarding with tongued and grooved joints to top rail and stiles and with inner edges of framing and abutting"]
[null,"edges of boarding chamfered to form V-joint","No",2]
[]
[null,"SECTION NO.3 BLOCK B, C AND D - ABLUTION BLOCKS"]
[]
[null,"BILL NO.4"]
[null,"PLUMBING AND DRAINAGE"]
[null,"PREAMBLES"]
[]
[null,"The  tenderer  is  referred  to  the  relevant  clauses  in  the"]
[null,"separate document Model Preambles for Trades  (2017"]
[null,"Edition) and to the Supplementary Preambles which are"]
[null,"incorporated in this Bill."]
[null,"_"]
[null,"PLUMBING AND DRAINAGE (PROVISIONAL)"]
[null,"RAINWATER DISPOSAL"]
[null,"0.6mm Chromadek seamless gutters and rainwater pipes"]
[]
[null,"155  x  100  x  115mm  aluminium  ogee  roof  gutters  with baked enamel finish fixed with concealed brackets","m",40]
[null,"Extra over gutter for stopped end","No",6]
[null,"75 x 100mm Diameter rainwater pipes","m",16]
[null,"Extra over gutter for outlet for 100 x 75mm pipe","No",6]
[null,"Extra  over  100mm  rainwater  pipe  for  eaves  or  plinth offset 650mm projection.","No",6]
[]
[null,"BUDGETARY ALLOWANCE"]
[null,"The  following  budgetary   allowance  for  plumbing"]
[null,"work, if required, to be executed by the contractor:"]
[null,"Provide  the  amount  of  R  60,  000.00  (Sixty  Thousand Rands) for plumbing work to be spent in whole or part or omitted from the contract. Work will be measured at scheduled rates.","item",1,60000]
[]
[null,"SECTION NO.3 BLOCK B, C AND D - ABLUTION BLOCKS"]
[]
[null,"BILL NO.5"]
[null,"TILING"]
[null,"PREAMBLES"]
[null,"The  tenderer  is  referred  to  the  relevant  clauses  in  the separate  document  Model  Preambles  for  Trades  (2017 Edition) and to the Supplementary Preambles which are incorporated in this Bill."]
[]
[null,"SUPPLEMENTARY PREAMBLES"]
[null,"Smooth,   off   form/shutter   or   power   floated   cement surfaces  must  be  acid  washed  to  remove  laitance  and rinsed with water\nNo  adhesive  is  to  be  applied  to  wet  screeds  nor  to screeds with a water content greater than that required by the adhesive manufacturer.\nLoading and heavy duty installations\nIn  areas  where  the  loading  exceeds  20kg/m²,  heavy traffic   areas   and   floor   areas   which   are   frequently washed  down  or  external  and  wet  conditions  flexible water resistant adhesives and grouts are recommended.\nPreparation of surfaces:\nOn  both  walls  and  floors  there  are  minimum  curing periods for walls and concrete floors as well as screeds and plasters and they are as follows:\nOn  both  walls  and  floors  there  are  minimum  curing periods for walls and concrete floors as well as screeds and plasters and they are as follows:\nSurfaces  must  be  firm  and  free  of  dust,  mould,  oil, grease, wax polish and organic growth. Organic growth must be removed and the spores killed with an effective fungicide such as a household bleaching solution."]
[]
[null,"Unless   described   as   fixed   with   adhesive   to   plaster (plaster  elsewhere),  descriptions  of  tiling  on  brick  or concrete   walls,   columns,   etc.,   shall   be   deemed   to include  1:4  cement  plaster  backing  and  descriptions  of tiling on concrete floors etc. shall be deemed to include 1:3 plaster bedding."]
[]
[null,"CERAMIC WALL TILING"]
[null,"Glazed ceramic wall tiles size 200 x 200 x 5mm thick fixed  with  Ceresit  Tylon  recommended  adhesive  or equal  and   approved   with  straight  joints   in   both directions,  jointed  and  flush  pointed  with  Ceresit Tylon CM33 white grout or equal and approved:"]
[]
[null,"On Walls (around Urinal)    ","m2",16]
[]
[null,"FLOOR TILING"]
[null,"600  x  600  x  10mm  Non  slip  glazed  floor  tiles  fixed with  high  strength  rapid  setting  adhesive  to  and plaster bedding on concrete ( elsewhere measured) and  flush  pointed  with  tinted  waterproof  jointing compound"]
[null," On floors and landings","m2",102]
[null,"Extra over tiles to floors for work done in patterns","m2",20]
[null,"100mm High cut tile","m",38]
[]
[null,"SECTION NO.3 BLOCK B, C AND D - ABLUTION BLOCKS"]
[null,"BILL NO.6"]
[null,"PAINTWORK"]
[null,"PREAMBLES"]
[null,"The  tenderer  is  referred  to  the  relevant  clauses  in  the separate  document  Model  Preambles  for  Trades  (2017 Edition) and to the Supplementary Preambles which are incorporated in this Bill.\n_\nSUPPLEMENTARY PREAMBLES"]
[null,"PAINT SPECIFICATIONS"]
[null,"All painting shall be done in accordance with \"Plascon\" specifications unless otherwise described\nPrime  all  skirtings  and  timber  work  not  visible  prior  to installation. Further  paint  all  glazing  beads  and  reveals prior to glazing.\nPrimers  and  first  coats  may  be  thinned  in  accordance with the paint specifications to aid the absorption of the paint.\nWhere  surfaces  of  plaster  etc  are  sandy  /  friable,  the first  coat  must  be  replaced  with  'Merit'  plaster  primer thinned 10% with turpentine.\nAll surfaces must be sound, clean and have a moisture content  of less than 8% for walls generally and 3% for slabs/screeds etc.\nThe  paint  and  surface  finishes  specified  herein  are  for normal  applications  as  intended  by  the  manufacturer. Should a finish be required for a surface other than that\nfor  which  it  would  normally  be  used,  then  the  specifier should contact manufacturer for approval."]
[]
[null,"Unless   otherwise   described   all   paintwork   shall   be deemed  to  have  a  colour  value  in  excess  of  7  on  the Munsell system in accordance with SANS 1091"]
[]
[null,"PAINTWORK ETC."]
[null,"ON INTERNAL FLOATED PLASTER SURFACES"]
[null,"Prepare  surfaces   and  remove  all  loose  material, apply  one  coat  'Plascon  Wall  and  All  Pure  Acrylic' thinned  20%  and  one  coat  'Plascon  Wall  and   All Pure Acrylic' paint or equal and approved:"]
[null," On internal walls","m2",271]
[null,"External walls","m2",200]
[]
[null,"ON WOOD"]
[null,"Stop,  sand  down  and  prepare  wood  surfaces  and apply one coat wood primer, one undercoat and two coats high gloss enamel paint:"]
[null,"On doors","m2",86]
[]
[null,"ON METAL"]
[null,"Prepare  surfaces  and  remove  all  loose   material, dust,   grease,   salts    and   contamination   with    a degreaser,   rinse   and   apply   one   coat   Calcium Plumbate Primer, one coat Universal Undercoat and two  coats  High  Gloss  Enamel  paint  on  galvanised steel:"]
[null,"On door frames","m2",9]
[null,"On window frames","m2",19]
[]
[null,"ON FIBRE-CEMENT"]
[null,"Apply  Plascon  meit  plaster  primer  and  two  coats Plascon Velvaglo Polyurethane Enamel paint."]
[null,"Fascias and barge boards","m",24]
[]
["SECTION SUMMARY - BLOCK B , C AND D - ABLUTION BLOCKS"]
[null,"Alterations and Demolitions"]
[]
[null,"Roof Coverings"]
[]
[null,"Carpentry and Joinery"]
[]
[null,"Plumbing and Drainage"]
[]
[null,"Tiling"]
[]
[null,"Paintwork"]
[]
[null,"SECTION NO. 4 CLASSROOM BLOCK, ADMIN OFFICE AND STUFF OFFICE"]
[null,"BILL NO.1"]
[null,"ALTERATIONS AND DEMOLITIONS"]
[null,"PREAMBLES"]
[null,"The  tenderer  is  referred  to  the  relevant  clauses  in  the separate  document  Model  Preambles  for  Trades  (2017 Edition) and to the Supplementary Preambles which are incorporated in this Bill."]
[]
[null,"SUPPLEMENTARY PREAMBLES"]
[null,"Damage and Repairs to Services\nShould the Contractor damage  any services which  are to  remain  in  operation  or  any  services  which  have  not yet   been   disconnected   prior   to   removal,   then   the Contractor   will   be   held   soley   responsible   for   such damage and any further resultant damage.\nThe     Contractor     shall     immediately     notify     the Representative/Agent   and   the   Authorities   concerned and   he   shall   at   his   own   cost   make   all   necessary arrangements  for  disconnection  and  repairs  with  the relevant  Authorities  and  shall pay  all  fees  and  charges levied.\nDisposal of Materials\nAll   existing   materials   specified   to    be   \"removed\", demolished   and   removed\",   \"hacked   up   or   off   and removed\",   or   \"taken   down   or   off   and  removed\"   or \"broken down and removed\", etc., become the property of the contractor. These materials and all debris, rubbish and  earth  must  be  carted  away  by  the  Contractor  and the  site  must  be  left  clean  and  unencumbered.  The Contractor   must   make   his   own   arrangements   for\ndumping and shall pay all fees and charges levied."]
[]
[null,"If  any  of  the  bricks  or  other  materials  specified  to  be \"removed\"  are  sound  and  considered  suitable  for  any portion   of   the   new   work   they   must   be   thoroughly cleaned  off  and  stacked  on  site  for  inspection  by  the Representative/Agent must be obtained before any such materials are re-used in the new work.\nAll  existing  materials  specified  to  be  \"taken  down  and set aside for re-use\" or \"taken down and set aside\" shall remain  the  property  of  Employer  and  must  be  cleaned off,  cleared  off  all  nails,  etc.  and  neatly  stacked  and stored  on  site  by  the  Contractor  where  directed  and carefully  handled  during taking down,  sotorage and re- fixing.  The  Contractor  will  be  held  responsible  for  the safety  of  these  materials  and  must  take  all  necessary precautions for their protection and any damage or loss that may occur must be made good by the Contractor at his own expense.\nThe Contractor must visit the site and the buildings and aquaint   himself   fully   with   conditions   and   scope   of alterations and demolitions. Descriptions herein are brief and  are  to  serve  as  a  means  of  identifying  work  only. The   full   extent   of   work   is   to   be   assessed   by   the contractor on site. All sizes indicated are approximate.\nRates  for  demolitions  and  alterations  are  to  include  for all  needling,  strutting  and  shoring,  etc.  that  may  be necessary whilst carrying out any portion of the work to ensure  the  stability  of  the  building  with  suitable  and substantial    materials    to    the    satisfaction    of    the Representatitve/Agent and remove when directed.\nOld Materials to become the property of the contractor."]
[]
[null,"Old  materials from  alterations, except where  described to be  re-used  or  handed  over,  become  the property  of the   contractor   who   must   allow   credit   in   the   final summary.\nOld Materials to be carted away:"]
[]
[null,"Old  materials from  alterations, except where  described to  be  re-used  or  handed  over,  as  well  as  rubbish,  etc. must be regularly carted from site and not to be allowed\nto accumulate on or around the site."]
[]
[null,"Handling over of materials"]
[null,"Where  certain  materials  or  articles  from  alterations  are described  to  be  handed  over  by  the  contractor  to  the Regional    Representative/Agent,    such    materials    or articles  shall  be  properly  stored  by  the  contractor,  until handling over thereof.\nThe Contractor must obtain an official receipt listing the materials  or  articles  and  dates  of  handing  over.  If  the contractor fails to submit the receipt when requested to do so,  it  shall be  deemed  that  the  materials  or  articles are  still  in  his  possession  and  he  will  be  held  liable  to the  Municipality  for  the  full  replacement  value  thereof, which  will  be  deducted  from  any  monies  due  to  the Contractor"]
[]
[null,"TEMPORARY BARRIERS, SCREENS, ETC."]
[null,"Temporary barriers, screens, etc. and including removal"]
[null,"Provide,  fix,  maintain,  move  and  subsequently  remove all  temporary  barriers,  screens,  overhead  projections, etc.  that  may  be  necessary  whilsy  carrying  out  any portion of the work for the protection of persons, animals and things, including the protection of existing buildings, structures, pavings and services on the remainder of the\nsite","item"]
[]
[null,"REMOVAL OF EXISTING WORK"]
[null,"Taking down and removing roofs, floors, panelling, ceilings, partitions, etc"]
[null,"RhinoBoard ceiling, including cornices, timber brandering, etc","m2",345]
[]
[null,"Taking up and removing wood block floor coverings, vinyl floor coverings, carpets, etc and preparing screeds for new floor coverings"]
[null,"Vinyl tile floor covering","m2",345]
[]
[null,"DEMOLITIONS"]
[null,"Allow for demolishing the existing strong room and take out carefully, the door, store for later use.","item",1]
[]
[null,"CRACKS REPAIRS"]
[null,"Allow  for  the  amount  of  R30,000.00  (Thirty  thousand Rand)   for   the   repairs   of   cracks   in   accordance   to Structural Engineers Instruction."]
[null,"Remove existing chakboard"]
[null,"Chalkboard","No",4]
[]
[null,"PREPARATORY WORK TO EXISTING SURFACES\n'Sika repair system' or similar approved"]
[]
[null,"Repair concrete surface with SIKA monotop 615 on SIKA monotop primer, then seal with SIKAFLEX, as per Repair concrete surface with SIKA monotop 615 on SIKA monotop primer, then seal with SIKAFLEX, as per manufacture's specification","m2",345]
[]
[null,"MAKING GOOD OF FINISHES, ETC"]
[null,"Making good"]
[null,"Make good screed to floors to receive new floor\ncoverings (elsewhere) ","m2",345]
[]
[null,"SECTION NO. 4 CLASSROOM BLOCK, ADMIN OFFICE AND STUFF OFFICE"]
[null,"BILL NO.2"]
[null,"ROOF COVERINGS, ETC."]
[null,"PREAMBLES"]
[]
[null,"The  tenderer  is  referred  to  the  relevant  clauses  in  the separate document Model Preambles for Trades  (2017 Edition) and to the Supplementary Preambles which are incorporated in this Bill."]
[]
[null,"SERVICE, REPAIRS, ETC. TO EXISTING"]
[null,"WORKS"]
[]
[null,"Service, repair and make good existing roof coverings"]
[]
[null,"Service  and  make  good  the  existing  roof  coverings including   refixing   roof   sheets   with   new   galvanised screws, patching all roof leaks with derbigum and leave roof  in  fully  functional  state  for  end  user.  (Provisional)\n(All leaking roofs iBlocks B, C and D","m2",345]
[]
[null,"SECTION NO. 4 CLASSROOM BLOCK, ADMIN OFFICE AND STUFF OFFICE"]
[null,"BILL NO.3"]
[null,"CARPENTRY AND JOINERY"]
[null,"PREAMBLES"]
[null,"The  tenderer  is  referred  to  the  relevant  clauses  in  the separate  document  Model  Preambles  for  Trades  (2017 Edition) and to the Supplementary Preambles which are incorporated in this Bill."]
[]
[null,"Fixing:\nItems  described  as  nailed  shall  be  deemed  to be  fixed with  hardened  stainless  steel  nails/slots  pins/spinless screws to brick or concrete.\nFixing brackets to be hot dipped galvanised where items not specifically mentioned.\nItems   described   as   \"plugged\"   shall   be   deemed   to include  screwing  to  fibre,  plastic  or  metal  plugs  at  not exceeding  500mm  centres,  and  where  described  as \"bolted\", the bolts have been given elsewhere\nDecorative thermosetting plastic laminate covering"]
[]
[null,"Laminate  covering  shall  be  glued  under  pressure  and edge  strips  of  same  shall  be  butt  jointed  at  junctions with adjacent similar finish"]
[]
[null,"EAVES, VERGES, ETC"]
[null,"'Everite Nutech'' Medium density fibre-cement facia board with H-profile plastic fascia jointers"]
[null,"12  x  225mm  Fascia  boards,  including  aluminium  H- profile   fascia   joiners    and   fixed   with   hot    dipped galvanised drive screws and washers (no paint) (Everite\nNutech - product number 041-203 and 685-195)","m",93]
[]
[null,"''Everite Nutech'' Fibre-cement socketless barge boards"]
[null,"10 x 80 x 225mm Barge boards including aluminium H- profile    barge    joiners    and   fixed    with    hot    dipped galvanised drive screws and washers (no paint) (Everite Nutech - product number 721-800)","m",18]
[]
[null,"DOORS, ETC."]
[null,"Refer to Architectural door schedule. \"Saligna Blaco\""]
[null,"40mm  Framed  ledged  and  braced  batten  door  813  x 2032mm high with 40 x 110mm styles and top rail, 20 x 150mm middle ledge, 20 x 225mm bottom ledge and 20 x 110mm braces filled in with V-jointed one side vertical boarding with tongued and grooved joints to top rail and stiles and with inner edges of framing and abutting edges of boarding chamfered to form V-joint (D1)","No",6]
[]
[null,"SKIRTINGS"]
[null,"Wrought meranti"]
[null,"19 x 76mm Skirtings with 19mm quadrant bead, plugged ","m",220]
[]
[null,"SECTION NO. 4 CLASSROOM BLOCK, ADMIN OFFICE AND STUFF OFFICE"]
[null,"BILL NO.4"]
[null,"CEILINGS, PARTITIONS AND ACCESS FLOORING"]
[null,"PREAMBLES"]
[null,"The  tenderer  is  referred  to  the  relevant  clauses  in  the separate  document  Model  Preambles  for  Trades  (2017 Edition) and to the Supplementary Preambles which are incorporated in this Bill.\n_\nSUPPLEMENTARY PREAMBLES"]
[]
[null,"Fixing\nItems described as \"nailed\" shall be deemed to be fixed with hardened steel nails  or pins, or to be shot-pinned, to brickwork or concrete\nItems   described   as   \"plugged\"   shall   be   deemed   to include  screwing  to  fibre,  plastic  or  metal  plugs  at  not exceeding  500mm  centres,  and  where  described  as \"bolted\", the bolts have been given elsewhere\nCeilings"]
[]
[null,"Unless otherwise described ceilings shall be deemed to be horizontal"]
[]
[null,"CEILINGS, ETC."]
[null,"NAILED-UP CEILINGS"]
[]
[null,"6.5mm Gypsum plasterboard with H-profile metal steel jointing strips"]
[null,"Ceilings including 50 x 50mm sawn softwood brandering at  400mm  centres  generally  in  one  direction  and  50  x 50mm branders and cross branders at joints and edges","m2",345]
[null,"of boards"]
[]
[null,"Extra  over  ceiling  for  600  x  600mm  trap  door  of  38  x 114mm   softwood   rebated   framing   with   one   cross brander,  covered  with  ceiling  board  and  fitted  flush  in\nopening, including necessary trimmers around","No",5]
[]
[null,"\"Rhino\" gypsum plasterboard cornices"]
[null,"5mm Coved cornices ","m",220]
[]
[null,"\"Isotherm\" insulation\n"]
[null,"50mm   Insulation   closely  fitted   and   laid   on   top   of brandering between roof timbers, etc ","m2",345]
[]
[null,"SECTION NO. 4 CLASSROOM BLOCK, ADMIN OFFICE AND STUFF OFFICE"]
[null,"BILL NO.5"]
[null,"FLOOR COVERINGS, PLASTIC LININGS, ETC."]
[null,"PREAMBLES"]
[null,"The  tenderer  is  referred  to  the  relevant  clauses  in  the separate  document  Model  Preambles  for  Trades  (2017 Edition) and to the Supplementary Preambles which are incorporated in this Bill."]
[]
[null,"SUPPLEMENTARY PREAMBLES"]
[null,"Fixing"]
[null,"Floor coverings, wall linings, etc shall, where applicable, be   fixed   with   adhesive   as   recommended   by   the manufacturers of the flooring, linings, etc"]
[]
[null,"FLOOR COVERINGS"]
[null,"VINYL FLOOR COVERINGS"]
[]
[null,"2mm thick x 1200mm wide Superflex fully flexible vinyl floor tiles","m2",345]
[null,"On floors"]
[]
[null,"POLISH, SEALERS, ETC"]
[null,"Three coats waterbased sealer on vinyl flooring.","m2",345]
[]
[null,"SECTION NO. 4 CLASSROOM BLOCK, ADMIN OFFICE AND STUFF OFFICE"]
[null,"BILL NO.6"]
[null,"IRONMONGERY"]
[null,"PREAMBLES"]
[null,"The  tenderer  is  referred  to  the  relevant  clauses  in  the separate document Model Preambles for Trades  (2017 Edition) and to the Supplementary Preambles which are incorporated in this Bill."]
[]
[]
[null,"LOCKS"]
[null,"\"Dorma\" or similar approved"]
[null,"\"Ref 390/313\" four-lever mortice lockset","No",6]
[]
[null,"SUNDRIES"]
[null,"38mm Diameter rubber door stop plugged","No",6]
[]
[null,"KEY TAGS"]
[null,"28mm  Diameter  x  1mm  thick  brass  key  tags  with  one numeral and one letter engraved","No",6]
[]
[null,"Approved standard stainless steel key rings","No",6]
[]
[null,"WRITING BOARDS, ETC"]
[null," \"Parrot\" or equal approved"]
[null,"Model  2203  white  vitreous   enamelled  wall  mounted white   board   2400   x   900mm   high   complete   with aluminium pen rail etc fixed to brickwork or partition system ( Magnetic)",null,6]
[]
[null,"EP09  Floortime domestic  pinning  boards  fixed  to brickwall strictly  in  accordance  to  manufacturer's instructions"]
[null,"2400 x 1200mm high pinning board fixed 900mm above finished floor level","No",6]
[]
[null,"Green   chalkboard  to   comply   with   CKS-38-1980 complete with chalk rail fixed in accordance with the manufacturers specifications","No",4]
[]
[]
[null,"SECTION NO.4\nBLOCK E - 4 CLASSROOM BLOCK, ADMIN OFFICE AND STUFF OFFICE\nBILL NO.7\nMETALWORK\nPREAMBLES\nThe tenderer is referred to the relevant clauses in the separate document Model Preambles for Trades (2017 Edition) and to the Supplementary Preambles which are incorporated in this Bill.\n_\nSUPPLEMENTARY PREAMBLES\nDescriptions of bolts, anchors, etc\nDescriptions of bolts shall be deemed to include nuts and washers\nDescriptions of expansion anchors and bolts and chemical anchors and bolts shall be deemed to include nuts, washers and mortices in brickwork or concrete\nItems described as \"holed for bolt(s)\" shall be deemed to exclude the bolts unless otherwise described\nItems described as \"plugged\" shall be deemed to include screwing to fibre, plastic or metal plugs at not exceeding 600mm centres"]
[]
[null,"STRONG ROOM DOOR"]
[null,"Take from store and install in position steel strong room door (Labour Only)","Item"]
[]
[null,"SECTION NO.4"]
[null,"BLOCK E - 4 CLASSROOM BLOCK, ADMIN OFFICE AND STUFF OFFICE"]
[]
[null,"BILL NO.8\nPLASTERING\nPREAMBLES\nThe tenderer is referred to the relevant clauses in the separate document Model Preambles for Trades (2017 Edition) and to the Supplementary Preambles which are incorporated in this Bill."]
[]
[null,"SCREEDS\nScreeds on concrete:"]
[null,"30mm Thick on floors.","m2",345]
[]
[null,"SECTION NO.4"]
[null,"BLOCK E - 4 CLASSROOM BLOCK, ADMIN OFFICE AND STUFF OFFICE"]
[]
[null,"BILL NO.9\nGLAZING\nPREAMBLES\nThe tenderer is referred to the relevant clauses in the separate document Model Preambles for Trades (2017 Edition) and to the Supple"]
[]
[null,"GLAZING TO STEEL WITH PUTTY"]
[null,"6mm Clear float glass\n\nPanes exceeding 0,1m2 and not exceeding 0,5m2","m2",65]
[]
[null,"SECTION NO.4"]
[]
[null,"BLOCK E - 4 CLASSROOM BLOCK, ADMIN\nOFFICE AND STUFF OFFICE"]
[]
[null,"BILL NO.10"]
[null,"PLUMBING AND DRAINAGE"]
[null,"PREAMBLES\nThe tenderer is referred to the relevant clauses in the\nseparate document Model Preambles for Trades (2017\nEdition) and to the Supplementary Preambles which are\nincorporated in this Bill."]
[]
[null,"PLUMBING AND DRAINAGE (PROVISIONAL)"]
[]
[null,"RAINWATER DISPOSAL"]
[null,"0.6mm Chromadek seamless gutters and rainwater pipes"]
[]
[null,"155 x 100 x 115mm aluminium ogee roof gutters with baked enamel finish fixed with concealed brackets","m",93]
[]
[null,"Extra over gutter for stopped end","No",4]
[]
[null,"75 x 100mm Diameter rainwater pipes","m",21]
[]
[null,"Extra over gutter for outlet for 100 x 75mm pipe","No",8]
[]
[null,"Extra over 100mm rainwater pipe for eaves or plinth offset 650mm projection.","No",8]
[]
[null,"FIRE APPLAINCES, ETC"]
[null,"\"Chubb\" or other equal and approved fire\nappliances all to SABS 543 requirements"]
[]
[null,"4.5kg Dry chemical powder portable fire extinguisher","no",3]
[]
[null,"190 x 190mm ABS plastic symbolic safety sign type FB2 plugged and screwed to wall.","no",3]
[]
[null,"RAINWATER TANK"]
[null,"Plastic \"JOJO\" Rainwater Tank"]
[]
[null,"Water plastic storage tank with the capacity of 2500 litres complete with access lid with inlet hole placed in position om concrete slab and anchored with and including four 7mm diameter galvanised steel chain anchors fitted into garden hose protective sleeves including cobra standard brass hose bibtap.","no",1]
[]
[]
[null,"SECTION NO.4"]
[null,"BLOCK E - 4 CLASSROOM BLOCK, ADMIN OFFICE AND STUFF OFFICE"]
[]
[null,"BILL NO.11"]
[]
[null,"PAINTWORK"]
[null,"\nThe tenderer is referred to the relevant clauses in the separate document Model Preambles for Trades (2017 Edition) and to the Supplementary Preambles which are incorporated in this Bill."]
[]
[null,"SUPPLEMENTARY PREAMBLES\nPAINT SPECIFICATIONS\nAll painting shall be done in accordance with \"Plascon\" specifications unless otherwise described\nPrime all skirtings and timber work not visible prior to installation. Further paint all glazing beads and reveals prior to glazing.\nPrimers and first coats may be thinned in accordance with the paint specifications to aid the absorption of the paint.\nWhere surfaces of plaster etc are sandy / friable, the first coat must be replaced with 'Merit' plaster primer thinned 10% with turpentine.\nAll surfaces must be sound, clean and have a moisture content of less than 8% for walls generally and 3% for slabs/screeds etc.\nThe paint and surface finishes specified herein are for normal applications as intended by the manufacturer. Should a finish be required for a surface other than that for which it would normally be used, then the specifier should contact manufacturer for approval."]
[]
[null,"COLOURS\nUnless otherwise described all paintwork shall be deemed to have a colour value in excess of 7 on the Munsell system in accordance with SANS 1091"]
[]
[null,"PAINTWORK ETC."]
[null,"ON INTERNAL FLOATED PLASTER SURFACES\nPrepare surfaces and remove all loose material, apply one coat 'Plascon Wall and All Pure Acrylic' thinned 20% and one coat 'Plascon Wall and All Pure Acrylic' paint or equal and approved:"]
[]
[null,"On internal walls.","m2",480]
[]
[null,"External walls","m2",284]
[]
[null,"ON PLASTERBOARD\nPrepare surfaces and remove all loose material, apply one coat 'Merit Plaster Primer' and two coats 'Plascon Double Velvet Pure Acrylic' paint or equal and approved:"]
[]
[null,"On ceilings and cornices.","m2",345]
[]
[null,"ON METAL"]
[null,"Prepare surfaces and remove all loose material, dust, grease, salts and contamination with a degreaser, rinse and apply one coat Calcium Plumbate Primer, one coat Universal Undercoat and two coats High Gloss Enamel paint on galvanised steel:"]
[]
[null,"On door frames","m2",18]
[]
[null,"On gates","m2",20]
[]
[null,"ON WOOD"]
[null,"Stop, sand down and prepare wood surfaces and apply one coat wood primer, one undercoat and two coats high gloss enamel paint:"]
[]
[null,"On doors","m2",20]
[]
[null,"ON FIBRE-CEMENT"]
[null,"Apply Plascon meit plaster primer and two coats Plascon Velvaglo Polyurethane Enamel paint."]
[]
[null,"Fascias and barge boards.","m",107]
[]
["SECTION SUMMARY - BLOCK E - 4 CLASSROOM BLOCK, ADMIN OFFICE A"]
[]
[null,"Alterations and Demolitions",61]
[]
[null,"Roof Coverings",62]
[]
[null,"Carpentry and Joinery",64]
[]
[null,"Ceilings, Partitions and Access Flooring",66]
[]
[null,"Floor Coverings",67]
[]
[null,"Ironmonery",69]
[]
[null,"Metalwork",70]
[]
[null,"Plastering",71]
[]
[null,"Glazing",72]
[]
[null,"Plumbing and Drainga",74]
[]
[null,"Paintork",77]
[]
[null,"SECTION NO.5"]
[null,"BLOCK F - SNP KITCHEN"]
[]
[null,"BILL NO.1"]
[null,"ALTERATIONS AND DEMOLITIONS\nPREAMBLES\nThe tenderer is referred to the relevant clauses in the separate document Model Preambles for Trades (2017 Edition) and to the Supplementary Preambles which are incorporated in this Bill."]
[]
[null,"SUPPLEMENTARY PREAMBLES\nDamage and Repairs to Services\nShould the Contractor damage any services which are to remain in operation or any services which have not yet been disconnected prior to removal, then the Contractor will be held soley responsible for such damage and any further resultant damage.\nThe Contractor shall immediately notify the Representative/Agent and the Authorities concerned and he shall at his own cost make all necessary arrangements for disconnection and repairs with the relevant Authorities and shall pay all fees and charges levied.\nDisposal of Materials\nAll existing materials specified to be \"removed\", demolished and removed\", \"hacked up or off and removed\", or \"taken down or off and removed\" or \"broken down and removed\", etc., become the property of the contractor. These materials and all debris, rubbish and earth must be carted away by the Contractor and the site must be left clean and unencumbered. The Contractor must make his own arrangements for dumping and shall pay all fees and charges levied."]
[]
[null,"If any of the bricks or other materials specified to be \"removed\" are sound and considered suitable for any portion of the new work they must be thoroughly cleaned off and stacked on site for inspection by the Representative/Agent must be obtained before any such materials are re-used in the new work.\nAll existing materials specified to be \"taken down and set aside for re-use\" or \"taken down and set aside\" shall remain the property of Employer and must be cleaned off, cleared off all nails, etc. and neatly stacked and stored on site by the Contractor where directed and carefully handled during taking down, storage and re- fixing. The Contractor will be held responsible for the safety of these materials and must take all necessary precautions for their protection and any damage or loss that may occur must be made good by the Contractor at his own expense.\nThe Contractor must visit the site and the buildings and aquaint himself fully with conditions and scope of alterations and demolitions. Descriptions herein are brief and are to serve as a means of identifying work only. The full extent of work is to be assessed by the contractor on site. All sizes indicated are approximate.\nRates for demolitions and alterations are to include for all needling, strutting and shoring, etc. that may be necessary whilst carrying out any portion of the work to ensure the stability of the building with suitable and substantial materials to the satisfaction of the Representatitve/Agent and remove when directed.\nOld Materials to become the property of the contractor.\nOld materials from alterations, except where described to be re-used or handed over, become the property of the contractor who must allow credit in the final summary."]
[]
[null,"Old Materials to become the property of the contractor.\nOld materials from alterations, except where described to be re-used or handed over, become the property of the contractor who must allow credit in the final summary.\n"]
[]
[null,"Old Materials to be carted away:\nOld materials from alterations, except where described to be re-used or handed over, as well as rubbish, etc. must be regularly carted from site and not to be allowed to accumulate on or around the site."]
[]
[null,"Handling over of materials\nWhere certain materials or articles from alterations are described to be handed over by the contractor to the Regional Representative/Agent, such materials or articles shall be properly stored by the contractor, until handling over thereof.\nThe Contractor must obtain an official receipt listing the materials or articles and dates of handing over. If the contractor fails to submit the receipt when requested to do so, it shall be deemed that the materials or articles are still in his possession and he will be held liable to the Municipality for the full replacement value thereof, which will be deducted from any monies due to the Contractor."]
[]
[null,"TEMPORARY BARRIERS, SCREENS, ETC"]
[null,"Temporary barriers, screens, etc. and including removal"]
[]
[null,"Provide, fix, maintain, move and subsequently remove all temporary barriers, screens, overhead projections, etc. that may be necessary whilsy carrying out any portion of the work for the protection of persons, animals and things, including the protection of existing buildings, structures, pavings and services on the remainder of the site","item"]
[]
[null,"REMOVAL OF EXISTING WORK"]
[null,"Remove the gypsum board ceilings, cornices, including timber battens complete"]
[]
[null,"Ceilings","m2",92]
[]
[null,"Taking out and removing piping, sanitary fittings, etc including disconnecting piping from fittings and making good floor and wall finishes (making good tiling and paintwork elsewhere)"]
[]
[null,"Wash Trough","No",1]
[]
[null,"Taking out and removing, burglar proof, doors, ironmongery, windows, etc from existing brickwall"]
[]
[null,"813 x 2032mm High timber door","No",1]
[]
[null,"SECTION NO.5"]
[null,"BLOCK F - SNP KITCHEN"]
[]
[null,"BILL NO.2"]
[null,"ROOF COVERINGS, ETC."]
[]
[null,"PREAMBLES\nThe tenderer is referred to the relevant clauses in the\nseparate document Model Preambles for Trades (2017\nEdition) and to the Supplementary Preambles which are\nincorporated in this Bill."]
[]
[null,"SERVICE, REPAIRS, ETC. TO EXISTING\nWORKS"]
[]
[null,"Service, repair and make good existing roof\ncoverings"]
[]
[null,"Service and make good the existing roof coverings\nincluding refixing roof sheets with new galvanised\nscrews, patching all roof leaks with derbigum and leave roof in fully functional state for end user. (Provisional)","m2",63]
[]
[null,"SECTION NO.5"]
[null,"BLOCK F - SNP KITCHEN"]
[]
[null,"BILL NO.3"]
[null,"CARPENTRY AND JOINERY"]
[]
[null,"PREAMBLES\nThe tenderer is referred to the relevant clauses in the separate document Model Preambles for Trades (2017 Edition) and to the Supplementary Preambles which are incorporated in this Bill."]
[]
[null,"SUPPLEMENTARY PREAMBLES\nFixing:\nItems described as nailed shall be deemed to be fixed with hardened stainless steel nails/slots pins/spinless screws to brick or concrete.\nFixing brackets to be hot dipped galvanised where items not specifically mentioned.\nItems described as \"plugged\" shall be deemed to include screwing to fibre, plastic or metal plugs at not exceeding 500mm centres, and where described as \"bolted\", the bolts have been given elsewhere\nDecorative thermosetting plastic laminate covering\nLaminate covering shall be glued under pressure and edge strips of same shall be butt jointed at junctions with adjacent similar finish"]
[]
[null,"DOORS, ETC."]
[null,"Refer to Architectural door schedule"]
[]
[null,"\"Saligna Blaco\""]
[]
[null,"40mm Framed ledged and braced batten door 813 x 2032mm high with 40 x 110mm styles and top rail, 20 x 150mm middle ledge, 20 x 225mm bottom ledge and 20 x 110mm braces filled in with V-jointed one side vertical boarding with tongued and grooved joints to top rail and stiles and with inner edges of framing and abutting\nedges of boarding chamfered to form V-joint","no",1]
[]
[null,"SECTION NO.5"]
[]
[null,"BLOCK F - SNAP KITCHEN"]
[null,"BILL NO.4"]
[null,"CEILINGS, PARTITIONS AND ACCESS FLOORING"]
[]
[null,"PREAMBLES\nThe tenderer is referred to the relevant clauses in the separate document Model Preambles for Trades (2017 Edition) and to the Supplementary Preambles which are incorporated in this Bill."]
[]
[null,"SUPPLEMENTARY PREAMBLES\nFixing\nItems described as \"nailed\" shall be deemed to be fixed with hardened steel nails or pins, or to be shot-pinned, to brickwork or concrete\nItems described as \"plugged\" shall be deemed to include screwing to fibre, plastic or metal plugs at not exceeding 500mm centres, and where described as \"bolted\", the bolts have been given elsewhere\nCeilings\nUnless otherwise described ceilings shall be deemed to be horizontal"]
[]
[null,"CEILINGS, ETC."]
[null,"NAILED-UP CEILINGS"]
[null,"6.5mm Gypsum plasterboard with H-profile metal steel jointing strips"]
[]
[null,"Ceilings including 50 x 50mm sawn softwood brandering at 400mm centres generally in one direction and 50 x 50mm branders and cross branders at joints and edges\nof boards","m2",92]
[]
[null,"Extra over ceiling for 600 x 600mm trap door of 38 x 114mm softwood rebated framing with one cross brander, covered with ceiling board and fitted flush in\nopening, including necessary trimmers around","no",1]
[]
[null,"\"Rhino\" gypsum plasterboard cornices"]
[null,"75mm Coved cornices","m",32]
[]
[null,"\"Isotherm\" insulation"]
[null,"50mm Insulation closely fitted and laid on top of brandering between roof timbers, etc","m2",92]
[]
[null,"SECTION NO.5"]
[null,"BLOCK F - SNP KITCHEN"]
[]
[null,"BILL NO.5"]
[null,"IRONMONGERY"]
[]
[null,"PREAMBLES\nThe tenderer is referred to the relevant clauses in the\nseparate document Model Preambles for Trades (2017\nEdition) and to the Supplementary Preambles which are\nincorporated in this Bill."]
[]
[null,"LOCKS"]
[null,"\"Dorma\" or similar approved"]
[]
[null,"\"Ref 390/313\" four-lever mortice lockset","no",1]
[]
[null,"SUNDRIES"]
[null,"38mm Diameter rubber door stop plugged","no",1]
[]
[null,"KEY TAGS"]
[null,"28mm Diameter x 1mm thick brass key tags with one numeral and one letter engraved","no",1]
[]
[null,"Approved standard stainless steel key rings","no",1]
[]
[null,"SECTION NO.5"]
[null,"BLOCK F - SNP KITCHEN"]
[]
[null,"BILL NO.6"]
[null,"PLUMBING AND DRAINAGE"]
[]
[null,"PREAMBLES\nThe tenderer is referred to the relevant clauses in the separate document Model Preambles for Trades (2008 Edition) and to the Supplementary Preambles which are incorporated in this Bill."]
[]
[null,"SUPPLEMENTARY PREAMBLES\nCopper pipes:\nPipes shall be hard drawn and half-hard pipes of the class stated. Class 0 (thin walled hard drawn) pipes shall not be bent. Class 1 (thin walled half-hard), class 2 (half-hard) and class 3 (heavy walled half-hard) pipes shall only be bent with benders with inner and outer formers. Fittings to copper waste, vent and anti-syphon pipes, capillary solder fittings and compression fittings shall be 'Cobra Watertech' type. Capillary solder fittings shall be 'Cobra Watertech' type. Capillary solder fittings shall comply with ISO 2016. Only compression fittings shall be used in walls or in ground.\nReducing fittings:\nWhere fittings have reducing ends or branches they are described as 'reducing'. In the case of pipes with diameters not exceeding 60mm only the largest end or branch size is given. Should the Contractor wish to use other fittings and bushes or reducers he may do so on the undertanding that no claim in this regard will be entertained. In the case of pipes with diameters exceeding 60mm all sizes are given and no claim for extra bushes, reducers, etc. will be entertained.\nWaste unions:"]
[]
[null,"uPVC pipes and fittings:\nSoil, waste and vent pipes and fittings shall be solvent weld jointed.\nDescriptions of waste unions shall be deemed to include rubber or vulcanite plugs and chains fixed to fittings."]
[]
[null,"SANITARY FITTINGS"]
[null,"Supply and fix wash trough to match the existing:"]
[null,"Wash trough as per Architect's specifcations","no",1]
[]
[null,"GAS INSTALLATION"]
[null,"Allow for gas installations complete with all necessary accessories","item",1]
[]
[null,"Allow for supply and fit steel cylinder cages to accommodate three cylinders","item",1]
[]
[null,"SECTION NO.5"]
[null,"BLOCK F - SNP KITCHEN"]
[]
[null,"BILL NO.7"]
[null,"TILING"]
[]
[null,"PREAMBLES\nThe tenderer is referred to the relevant clauses in the separate document Model Preambles for Trades (2017 Edition) and to the Supplementary Preambles which are incorporated in this Bill."]
[]
[null,"SUPPLEMENTARY PREAMBLES\nSmooth, off form/shutter or power floated cement surfaces must be acid washed to remove laitance and rinsed with water\nNo adhesive is to be applied to wet screeds nor to screeds with a water content greater than that required by the adhesive manufacturer.\nLoading and heavy duty installations\nIn areas where the loading exceeds 20kg/m², heavy traffic areas and floor areas which are frequently washed down or external and wet conditions flexible water resistant adhesives and grouts are recommended.\nPreparation of surfaces:\nOn both walls and floors there are minimum curing periods for walls and concrete floors as well as screeds and plasters and they are as follows:\nOn both walls and floors there are minimum curing periods for walls and concrete floors as well as screeds and plasters and they are as follows:\nSurfaces must be firm and free of dust, mould, oil, grease, wax polish and organic growth. Organic growth must be removed and the spores killed with an effective fungicide such as a household bleaching solution."]
[]
[null,"Unless described as fixed with adhesive to plaster (plaster elsewhere), descriptions of tiling on brick or concrete walls, columns, etc., shall be deemed to include 1:4 cement plaster backing and descriptions of tiling on concrete floors etc. shall be deemed to include 1:3 plaster bedding."]
[]
[null,"FLOOR TILING"]
[null,"600 x 600 x 10mm Non slip glazed floor tiles fixed with high strength rapid setting adhesive to and plaster bedding on concrete ( elsewhere measured) and flush pointed with tinted waterproof jointing compound (Allow a Prime Cost Amount of R200.00/m2):"]
[]
[null,"On floors and landings","m2",92]
[]
[null,"Extra over tiles to floors for work done in patterns","m2",20]
[]
[null,"100mm High cut tile","m",32]
[]
[null,"SECTION NO.5"]
[null,"BLOCK E - SNP KITCHEN"]
[]
[null,"BILL NO.8"]
[null,"GLAZING"]
[null,"PREAMBLES\nThe tenderer is referred to the relevant clauses in the separate document Model Preambles for Trades (2017 Edition) and to the Supplementary Preambles which are incorporated in this Bill."]
[]
[null,"GLAZING TO STEEL WITH PUTTY"]
[]
[null,"6mm Clear float glass"]
[null,"Panes exceeding 0,1m2 and not exceeding 0,5m2","m2",13]
[]
[null,"SECTION NO.5"]
[null,"BLOCK G - GRADE R BLOCK"]
[]
[null,"BILL NO.9"]
[]
[null,"PAINTWORK"]
[null,"PREAMBLES\nThe tenderer is referred to the relevant clauses in the separate document Model Preambles for Trades (2017 Edition) and to the Supplementary Preambles which are incorporated in this Bill."]
[]
[null,"PAINT SPECIFICATIONS\nAll painting shall be done in accordance with \"Plascon\" specifications unless otherwise described\nPrime all skirtings and timber work not visible prior to installation. Further paint all glazing beads and reveals prior to glazing.\nPrimers and first coats may be thinned in accordance with the paint specifications to aid the absorption of the paint.\nWhere surfaces of plaster etc are sandy / friable, the first coat must be replaced with 'Merit' plaster primer thinned 10% with turpentine.\nAll surfaces must be sound, clean and have a moisture content of less than 8% for walls generally and 3% for slabs/screeds etc.\nThe paint and surface finishes specified herein are for normal applications as intended by the manufacturer. Should a finish be required for a surface other than that for which it would normally be used, then the specifier should contact manufacturer for approval."]
[]
[null,"COLOURS\nUnless otherwise described all paintwork shall be deemed to have a colour value in excess of 7 on the Munsell system in accordance with SANS 1091"]
[]
[null,"PAINTWORK ETC."]
[]
[null,"ON INTERNAL FLOATED PLASTER SURFACES"]
[null,"Prepare surfaces and remove all loose material, apply one coat 'Plascon Wall and All Pure Acrylic' thinned 20% and one coat 'Plascon Wall and All Pure Acrylic' paint or equal and approved:"]
[]
[null,"On internal walls.","m2",126]
[]
[null,"External walls","m2",86]
[]
[null,"ON METAL"]
[]
[null,"Prepare surfaces and remove all loose material, dust, grease, salts and contamination with a degreaser, rinse and apply one coat Calcium Plumbate Primer, one coat Universal Undercoat and two coats High Gloss Enamel paint on galvanised steel:"]
[]
[null,"On door frames","m2",4]
[]
[null,"On Windows","m2",26]
[]
[null,"On gates","m2",7]
[]
[null,"ON WOOD\nStop, sand down and prepare wood surfaces and apply one coat wood primer, one undercoat and two coats high gloss enamel paint:"]
[]
[null,"On doors","m2",10]
[]
[null,"ON FIBRE-CEMENT"]
[null,"Apply Plascon meit plaster primer and two coats Plascon Velvaglo Polyurethane Enamel paint."]
[]
[null,"Fascias and barge boards.","m",15]
[]
["SECTION SUMMARY - BLOCK F - SNP KITCHEN"]
[]
[null,"Alterations and Demolitions",81]
[]
[null,"Roof Coverings",82]
[]
[null,"Carpentry and Joinery",84]
[]
[null,"Ceilings, Partitions and Access Flooring",86]
[]
[null,"Ironmongery",87]
[]
[null,"Plumbing and Drainage",89]
[]
[null,"Tilling",91]
[]
[null,"Glazing",92]
[]
[null,"Paintwork",95]
[]
[]
[null,"SECTION NO. 6 GRADE R BLOCK"]
[null,"BILL NO.1"]
[null,"ALTERATIONS AND DEMOLITIONS"]
[null,"PREAMBLES"]
[null,"The  tenderer  is  referred  to  the  relevant  clauses  in  the separate  document  Model  Preambles  for  Trades  (2017 Edition) and to the Supplementary Preambles which are incorporated in this Bill."]
[]
[null,"SUPPLEMENTARY PREAMBLES"]
[null,"Damage and Repairs to Services\nShould the Contractor damage  any services which  are to  remain  in  operation  or  any  services  which  have  not yet   been   disconnected   prior   to   removal,   then   the Contractor   will   be   held   soley   responsible   for   such damage and any further resultant damage.\nThe     Contractor     shall     immediately     notify     the Representative/Agent   and   the   Authorities   concerned and   he   shall   at   his   own   cost   make   all   necessary arrangements  for  disconnection  and  repairs  with  the relevant  Authorities  and  shall pay  all  fees  and  charges levied.\nDisposal of Materials\nAll   existing   materials   specified   to    be   \"removed\", demolished   and   removed\",   \"hacked   up   or   off   and removed\",   or   \"taken   down   or   off   and  removed\"   or \"broken down and removed\", etc., become the property of the contractor. These materials and all debris, rubbish and  earth  must  be  carted  away  by  the  Contractor  and the  site  must  be  left  clean  and  unencumbered.  The Contractor   must   make   his   own   arrangements   for\ndumping and shall pay all fees and charges levied."]
[]
[null,"If  any  of  the  bricks  or  other  materials  specified  to  be \"removed\"  are  sound  and  considered  suitable  for  any portion   of   the   new   work   they   must   be   thoroughly cleaned  off  and  stacked  on  site  for  inspection  by  the Representative/Agent must be obtained before any such materials are re-used in the new work.\nAll  existing  materials  specified  to  be  \"taken  down  and set aside for re-use\" or \"taken down and set aside\" shall remain  the  property  of  Employer  and  must  be  cleaned off,  cleared  off  all  nails,  etc.  and  neatly  stacked  and stored  on  site  by  the  Contractor  where  directed  and carefully  handled  during taking down,  sotorage and re- fixing.  The  Contractor  will  be  held  responsible  for  the safety  of  these  materials  and  must  take  all  necessary precautions for their protection and any damage or loss that may occur must be made good by the Contractor at his own expense.\nThe Contractor must visit the site and the buildings and aquaint   himself   fully   with   conditions   and   scope   of alterations and demolitions. Descriptions herein are brief and  are  to  serve  as  a  means  of  identifying  work  only. The   full   extent   of   work   is   to   be   assessed   by   the contractor on site. All sizes indicated are approximate.\nRates  for  demolitions  and  alterations  are  to  include  for all  needling,  strutting  and  shoring,  etc.  that  may  be necessary whilst carrying out any portion of the work to ensure  the  stability  of  the  building  with  suitable  and substantial    materials    to    the    satisfaction    of    the Representatitve/Agent and remove when directed.\nOld Materials to become the property of the contractor."]
[]
[null,"Old  materials from  alterations, except where  described to be  re-used  or  handed  over,  become  the property  of the   contractor   who   must   allow   credit   in   the   final summary.\nOld Materials to be carted away:"]
[]
[null,"Old  materials from  alterations, except where  described to  be  re-used  or  handed  over,  as  well  as  rubbish,  etc. must be regularly carted from site and not to be allowed\nto accumulate on or around the site."]
[]
[null,"Handling over of materials"]
[null,"Where  certain  materials  or  articles  from  alterations  are described  to  be  handed  over  by  the  contractor  to  the Regional    Representative/Agent,    such    materials    or articles  shall  be  properly  stored  by  the  contractor,  until handling over thereof.\nThe Contractor must obtain an official receipt listing the materials  or  articles  and  dates  of  handing  over.  If  the contractor fails to submit the receipt when requested to do so,  it  shall be  deemed  that  the  materials  or  articles are  still  in  his  possession  and  he  will  be  held  liable  to the  Municipality  for  the  full  replacement  value  thereof, which  will  be  deducted  from  any  monies  due  to  the Contractor"]
[]
[null,"TEMPORARY BARRIERS, SCREENS, ETC."]
[null,"Temporary barriers, screens, etc. and including removal"]
[null,"Provide,  fix,  maintain,  move  and  subsequently  remove all  temporary  barriers,  screens,  overhead  projections, etc.  that  may  be  necessary  whilsy  carrying  out  any portion of the work for the protection of persons, animals and things, including the protection of existing buildings, structures, pavings and services on the remainder of the\nsite","item"]
[]
[null,"REMOVAL OF EXISTING WORK"]
[null,"Taking down and removing roofs, floors, panelling, ceilings, partitions, etc"]
[]
[null,"Taking up and removing wood block floor coverings, vinyl floor coverings, carpets, etc and preparing screeds for new floor coverings"]
[null,"Vinyl tile floor covering","m2",173]
[]
[null,"Remove the gypsum board ceilings, cornices, including timber battens complete"]
[null,"Ceilings","m2",173]
[]
[null,"Taking out and removing doors, ironmongery"]
[null,"Timber single door including iromongery","No",2]
[]
[null,"Remove existing chakboard"]
[null,"Chalkboard","No",2]
[]
[]
[null,"PREPARATORY WORK TO EXISTING SURFACES\n'Sika repair system' or similar approved"]
[]
[null,"Repair concrete surface with SIKA monotop 615 on SIKA monotop primer, then seal with SIKAFLEX, as per Repair concrete surface with SIKA monotop 615 on SIKA monotop primer, then seal with SIKAFLEX, as per manufacture's specification","m2",173]
[]
[null,"MAKING GOOD OF FINISHES, ETC"]
[null,"Making good"]
[null,"Make good screed to floors to receive new floor\ncoverings (elsewhere) ","m2",173]
[]
[null,"SECTION NO. 6 GRADE R BLOCK"]
[null,"BILL NO.2"]
[null,"ROOF COVERINGS, ETC."]
[null,"PREAMBLES"]
[]
[null,"The  tenderer  is  referred  to  the  relevant  clauses  in  the separate document Model Preambles for Trades  (2017 Edition) and to the Supplementary Preambles which are incorporated in this Bill."]
[]
[null,"SERVICE, REPAIRS, ETC. TO EXISTING"]
[null,"WORKS"]
[]
[null,"Service, repair and make good existing roof coverings"]
[]
[null,"Service  and  make  good  the  existing  roof  coverings including   refixing   roof   sheets   with   new   galvanised screws, patching all roof leaks with derbigum and leave roof  in  fully  functional  state  for  end  user.  (Provisional)\n(All leaking roofs iBlocks B, C and D","m2",173]
[]
[null,"SECTION NO. 6 GRADE R BLOCK"]
[null,"BILL NO.3"]
[null,"CARPENTRY AND JOINERY"]
[null,"PREAMBLES"]
[null,"The  tenderer  is  referred  to  the  relevant  clauses  in  the separate  document  Model  Preambles  for  Trades  (2017 Edition) and to the Supplementary Preambles which are incorporated in this Bill."]
[]
[null,"Fixing:\nItems  described  as  nailed  shall  be  deemed  to be  fixed with  hardened  stainless  steel  nails/slots  pins/spinless screws to brick or concrete.\nFixing brackets to be hot dipped galvanised where items not specifically mentioned.\nItems   described   as   \"plugged\"   shall   be   deemed   to include  screwing  to  fibre,  plastic  or  metal  plugs  at  not exceeding  500mm  centres,  and  where  described  as \"bolted\", the bolts have been given elsewhere\nDecorative thermosetting plastic laminate covering"]
[]
[null,"Laminate  covering  shall  be  glued  under  pressure  and edge  strips  of  same  shall  be  butt  jointed  at  junctions with adjacent similar finish"]
[]
[null,"EAVES, VERGES, ETC"]
[null,"'Everite Nutech'' Medium density fibre-cement facia board with H-profile plastic fascia jointers"]
[null,"12  x  225mm  Fascia  boards,  including  aluminium  H- profile   fascia   joiners    and   fixed   with   hot    dipped galvanised drive screws and washers (no paint) (Everite\nNutech - product number 041-203 and 685-195)","m",46]
[]
[null,"''Everite Nutech'' Fibre-cement socketless barge boards"]
[null,"10 x 80 x 225mm Barge boards including aluminium H- profile    barge    joiners    and   fixed    with    hot    dipped galvanised drive screws and washers (no paint) (Everite Nutech - product number 721-800)","m",18]
[]
[null,"DOORS, ETC."]
[null,"Refer to Architectural door schedule. \"Saligna Blaco\""]
[null,"40mm  Framed  ledged  and  braced  batten  door  813  x 2032mm high with 40 x 110mm styles and top rail, 20 x 150mm middle ledge, 20 x 225mm bottom ledge and 20 x 110mm braces filled in with V-jointed one side vertical boarding with tongued and grooved joints to top rail and stiles and with inner edges of framing and abutting edges of boarding chamfered to form V-joint (D1)","No",2]
[]
[null,"SKIRTINGS"]
[null,"Wrought meranti"]
[null,"19 x 76mm Skirtings with 19mm quadrant bead, plugged ","m",76]
[]
[null,"SECTION NO. 6 GRADE R BLOCK"]
[null,"BILL NO.4"]
[null,"CEILINGS, PARTITIONS AND ACCESS FLOORING"]
[null,"PREAMBLES"]
[null,"The  tenderer  is  referred  to  the  relevant  clauses  in  the separate  document  Model  Preambles  for  Trades  (2017 Edition) and to the Supplementary Preambles which are incorporated in this Bill.\n_\nSUPPLEMENTARY PREAMBLES"]
[]
[null,"Fixing\nItems described as \"nailed\" shall be deemed to be fixed with hardened steel nails  or pins, or to be shot-pinned, to brickwork or concrete\nItems   described   as   \"plugged\"   shall   be   deemed   to include  screwing  to  fibre,  plastic  or  metal  plugs  at  not exceeding  500mm  centres,  and  where  described  as \"bolted\", the bolts have been given elsewhere\nCeilings"]
[]
[null,"Unless otherwise described ceilings shall be deemed to be horizontal"]
[]
[null,"CEILINGS, ETC."]
[null,"NAILED-UP CEILINGS"]
[]
[null,"6.5mm Gypsum plasterboard with H-profile metal steel jointing strips"]
[null,"Ceilings including 50 x 50mm sawn softwood brandering at  400mm  centres  generally  in  one  direction  and  50  x 50mm branders and cross branders at joints and edges","m2",173]
[null,"of boards"]
[]
[null,"Extra  over  ceiling  for  600  x  600mm  trap  door  of  38  x 114mm   softwood   rebated   framing   with   one   cross brander,  covered  with  ceiling  board  and  fitted  flush  in\nopening, including necessary trimmers around","No",2]
[]
[null,"\"Rhino\" gypsum plasterboard cornices"]
[null,"5mm Coved cornices ","m",76]
[]
[null,"\"Isotherm\" insulation\n"]
[null,"50mm   Insulation   closely  fitted   and   laid   on   top   of brandering between roof timbers, etc ","m2",173]
[]
[null,"SECTION NO. 6 GRADE R BLOCK"]
[null,"BILL NO.5"]
[null,"FLOOR COVERINGS, PLASTIC LININGS, ETC."]
[null,"PREAMBLES"]
[null,"The  tenderer  is  referred  to  the  relevant  clauses  in  the separate  document  Model  Preambles  for  Trades  (2017 Edition) and to the Supplementary Preambles which are incorporated in this Bill."]
[]
[null,"SUPPLEMENTARY PREAMBLES"]
[null,"Fixing"]
[null,"Floor coverings, wall linings, etc shall, where applicable, be   fixed   with   adhesive   as   recommended   by   the manufacturers of the flooring, linings, etc"]
[]
[null,"FLOOR COVERINGS"]
[null,"VINYL FLOOR COVERINGS"]
[]
[null,"2mm thick x 1200mm wide Superflex fully flexible vinyl floor tiles","m2",173]
[null,"On floors"]
[]
[null,"POLISH, SEALERS, ETC"]
[null,"Three coats waterbased sealer on vinyl flooring.","m2",173]
[]
[null,"SECTION NO. 6 GRADE R BLOCK"]
[null,"BILL NO.6"]
[null,"IRONMONGERY"]
[null,"PREAMBLES"]
[null,"The  tenderer  is  referred  to  the  relevant  clauses  in  the separate document Model Preambles for Trades  (2017 Edition) and to the Supplementary Preambles which are incorporated in this Bill."]
[]
[]
[null,"LOCKS"]
[null,"\"Dorma\" or similar approved"]
[null,"\"Ref 390/313\" four-lever mortice lockset","No",2]
[]
[null,"SUNDRIES"]
[null,"38mm Diameter rubber door stop plugged","No",2]
[]
[null,"KEY TAGS"]
[null,"28mm  Diameter  x  1mm  thick  brass  key  tags  with  one numeral and one letter engraved","No",2]
[]
[null,"Approved standard stainless steel key rings","No",2]
[]
[null,"WRITING BOARDS, ETC"]
[null," \"Parrot\" or equal approved"]
[null,"Model  2203  white  vitreous   enamelled  wall  mounted white   board   2400   x   900mm   high   complete   with aluminium pen rail etc fixed to brickwork or partition system ( Magnetic)","No",2]
[]
[null,"EP09  Floortime domestic  pinning  boards  fixed  to brickwall strictly  in  accordance  to  manufacturer's instructions"]
[null,"2400 x 1200mm high pinning board fixed 900mm above finished floor level","No",2]
[]
[null,"Green   chalkboard  to   comply   with   CKS-38-1980 complete with chalk rail fixed in accordance with the manufacturers specifications","No",2]
[]
[]
[]
[null,"SECTION NO.6"]
[null,"GRADE R BLOCK"]
[null,"PREAMBLES\nThe tenderer is referred to the relevant clauses in the\nseparate document Model Preambles for Trades (2017\nEdition) and to the Supplementary Preambles which are\nincorporated in this Bill."]
[]
[null,"PLUMBING AND DRAINAGE (PROVISIONAL)"]
[]
[null,"RAINWATER DISPOSAL"]
[null,"0.6mm Chromadek seamless gutters and rainwater pipes"]
[]
[null,"155 x 100 x 115mm aluminium ogee roof gutters with baked enamel finish fixed with concealed brackets","m",46]
[]
[null,"Extra over gutter for stopped end","No",4]
[]
[null,"75 x 100mm Diameter rainwater pipes","m",16]
[]
[null,"Extra over gutter for outlet for 100 x 75mm pipe","No",6]
[]
[null,"Extra over 100mm rainwater pipe for eaves or plinth offset 650mm projection.","No",6]
[]
[null,"FIRE APPLAINCES, ETC"]
[null,"\"Chubb\" or other equal and approved fire\nappliances all to SABS 543 requirements"]
[]
[null,"4.5kg Dry chemical powder portable fire extinguisher","no",2]
[]
[null,"190 x 190mm ABS plastic symbolic safety sign type FB2 plugged and screwed to wall.","no",2]
[]
[]
[null,"SECTION NO.6"]
[null,"GRADE R BLOCK"]
[]
[null,"BILL NO.8\nGLAZING\nPREAMBLES\nThe tenderer is referred to the relevant clauses in the separate document Model Preambles for Trades (2017 Edition) and to the Supple"]
[]
[null,"GLAZING TO STEEL WITH PUTTY"]
[null,"6mm Clear float glass\n\nPanes exceeding 0,1m2 and not exceeding 0,5m2","m2",19]
[]
[null,"SECTION NO.6"]
[]
[null,"GRADE R BLOCK"]
[]
[]
[]
[null,"SECTION NO.6"]
[null,"GRADE R BLOCK"]
[]
[null,"BILL NO.9"]
[]
[null,"PAINTWORK"]
[null,"\nThe tenderer is referred to the relevant clauses in the separate document Model Preambles for Trades (2017 Edition) and to the Supplementary Preambles which are incorporated in this Bill."]
[]
[null,"SUPPLEMENTARY PREAMBLES\nPAINT SPECIFICATIONS\nAll painting shall be done in accordance with \"Plascon\" specifications unless otherwise described\nPrime all skirtings and timber work not visible prior to installation. Further paint all glazing beads and reveals prior to glazing.\nPrimers and first coats may be thinned in accordance with the paint specifications to aid the absorption of the paint.\nWhere surfaces of plaster etc are sandy / friable, the first coat must be replaced with 'Merit' plaster primer thinned 10% with turpentine.\nAll surfaces must be sound, clean and have a moisture content of less than 8% for walls generally and 3% for slabs/screeds etc.\nThe paint and surface finishes specified herein are for normal applications as intended by the manufacturer. Should a finish be required for a surface other than that for which it would normally be used, then the specifier should contact manufacturer for approval."]
[]
[null,"COLOURS\nUnless otherwise described all paintwork shall be deemed to have a colour value in excess of 7 on the Munsell system in accordance with SANS 1091"]
[]
[null,"PAINTWORK ETC."]
[null,"ON INTERNAL FLOATED PLASTER SURFACES\nPrepare surfaces and remove all loose material, apply one coat 'Plascon Wall and All Pure Acrylic' thinned 20% and one coat 'Plascon Wall and All Pure Acrylic' paint or equal and approved:"]
[]
[null,"On internal walls.","m2",200]
[]
[null,"External walls","m2",161]
[]
[null,"ON PLASTERBOARD\nPrepare surfaces and remove all loose material, apply one coat 'Merit Plaster Primer' and two coats 'Plascon Double Velvet Pure Acrylic' paint or equal and approved:"]
[]
[null,"On ceilings and cornices.","m2",173]
[]
[null,"ON METAL"]
[null,"Prepare surfaces and remove all loose material, dust, grease, salts and contamination with a degreaser, rinse and apply one coat Calcium Plumbate Primer, one coat Universal Undercoat and two coats High Gloss Enamel paint on galvanised steel:"]
[]
[null,"On door frames","m2",3]
[]
[null,"On gates","m2",7]
[]
[null,"ON WOOD"]
[null,"Stop, sand down and prepare wood surfaces and apply one coat wood primer, one undercoat and two coats high gloss enamel paint:"]
[]
[null,"On doors","m2",7]
[]
[null,"ON FIBRE-CEMENT"]
[null,"Apply Plascon meit plaster primer and two coats Plascon Velvaglo Polyurethane Enamel paint."]
[]
[null,"Fascias and barge boards.","m",61]
[]
["SECTION SUMMARY - BLOCK G GRADE R BLOCK"]
[]
[null,"Alterations and Demolitions",100]
[]
[null,"Roof Coverings",101]
[]
[null,"Carpentry and Joinery",103]
[]
[null,"Ceilings, Partitions and Access Flooring",105]
[]
[null,"Floor Coverings",106]
[]
[null,"Ironmonery",108]
[]
[null,"Plumbing and Drainage",109]
[]
[null,"Glazing",110]
[]
[null,"Paintork",113]
[]
[]
[null,"SECTION NO.8 BLOCK H - 4 CLASSROOMS"]
[null,"BILL NO.1"]
[null,"ALTERATIONS AND DEMOLITIONS"]
[null,"PREAMBLES"]
[null,"The  tenderer  is  referred  to  the  relevant  clauses  in  the separate  document  Model  Preambles  for  Trades  (2017 Edition) and to the Supplementary Preambles which are incorporated in this Bill."]
[]
[null,"SUPPLEMENTARY PREAMBLES"]
[null,"Damage and Repairs to Services\nShould the Contractor damage  any services which  are to  remain  in  operation  or  any  services  which  have  not yet   been   disconnected   prior   to   removal,   then   the Contractor   will   be   held   soley   responsible   for   such damage and any further resultant damage.\nThe     Contractor     shall     immediately     notify     the Representative/Agent   and   the   Authorities   concerned and   he   shall   at   his   own   cost   make   all   necessary arrangements  for  disconnection  and  repairs  with  the relevant  Authorities  and  shall pay  all  fees  and  charges levied.\nDisposal of Materials\nAll   existing   materials   specified   to    be   \"removed\", demolished   and   removed\",   \"hacked   up   or   off   and removed\",   or   \"taken   down   or   off   and  removed\"   or \"broken down and removed\", etc., become the property of the contractor. These materials and all debris, rubbish and  earth  must  be  carted  away  by  the  Contractor  and the  site  must  be  left  clean  and  unencumbered.  The Contractor   must   make   his   own   arrangements   for\ndumping and shall pay all fees and charges levied."]
[]
[null,"If  any  of  the  bricks  or  other  materials  specified  to  be \"removed\"  are  sound  and  considered  suitable  for  any portion   of   the   new   work   they   must   be   thoroughly cleaned  off  and  stacked  on  site  for  inspection  by  the Representative/Agent must be obtained before any such materials are re-used in the new work.\nAll  existing  materials  specified  to  be  \"taken  down  and set aside for re-use\" or \"taken down and set aside\" shall remain  the  property  of  Employer  and  must  be  cleaned off,  cleared  off  all  nails,  etc.  and  neatly  stacked  and stored  on  site  by  the  Contractor  where  directed  and carefully  handled  during taking down,  sotorage and re- fixing.  The  Contractor  will  be  held  responsible  for  the safety  of  these  materials  and  must  take  all  necessary precautions for their protection and any damage or loss that may occur must be made good by the Contractor at his own expense.\nThe Contractor must visit the site and the buildings and aquaint   himself   fully   with   conditions   and   scope   of alterations and demolitions. Descriptions herein are brief and  are  to  serve  as  a  means  of  identifying  work  only. The   full   extent   of   work   is   to   be   assessed   by   the contractor on site. All sizes indicated are approximate.\nRates  for  demolitions  and  alterations  are  to  include  for all  needling,  strutting  and  shoring,  etc.  that  may  be necessary whilst carrying out any portion of the work to ensure  the  stability  of  the  building  with  suitable  and substantial    materials    to    the    satisfaction    of    the Representatitve/Agent and remove when directed.\nOld Materials to become the property of the contractor."]
[]
[null,"Old  materials from  alterations, except where  described to be  re-used  or  handed  over,  become  the property  of the   contractor   who   must   allow   credit   in   the   final summary.\nOld Materials to be carted away:"]
[]
[null,"Old  materials from  alterations, except where  described to  be  re-used  or  handed  over,  as  well  as  rubbish,  etc. must be regularly carted from site and not to be allowed\nto accumulate on or around the site."]
[]
[null,"Handling over of materials"]
[null,"Where  certain  materials  or  articles  from  alterations  are described  to  be  handed  over  by  the  contractor  to  the Regional    Representative/Agent,    such    materials    or articles  shall  be  properly  stored  by  the  contractor,  until handling over thereof.\nThe Contractor must obtain an official receipt listing the materials  or  articles  and  dates  of  handing  over.  If  the contractor fails to submit the receipt when requested to do so,  it  shall be  deemed  that  the  materials  or  articles are  still  in  his  possession  and  he  will  be  held  liable  to the  Municipality  for  the  full  replacement  value  thereof, which  will  be  deducted  from  any  monies  due  to  the Contractor"]
[]
[null,"TEMPORARY BARRIERS, SCREENS, ETC."]
[null,"Temporary barriers, screens, etc. and including removal"]
[null,"Provide,  fix,  maintain,  move  and  subsequently  remove all  temporary  barriers,  screens,  overhead  projections, etc.  that  may  be  necessary  whilsy  carrying  out  any portion of the work for the protection of persons, animals and things, including the protection of existing buildings, structures, pavings and services on the remainder of the\nsite","item"]
[]
[null,"REMOVAL OF EXISTING WORK"]
[null,"Taking down and removing roofs, floors, panelling, ceilings, partitions, etc"]
[]
[null,"Taking up and remove damaged fascia board"]
[null,"Fascia boards and bardge boards","m2",79]
[]
[null,"Take out timber doors including ironmongery"]
[null,"Single Door","m2",2]
[]
[null,"Remove existing chakboard"]
[null,"Chalkboard","No",4]
[]
[null,"PREPARATORY WORK TO EXISTING SURFACES\n'Sika repair system' or similar approved"]
[]
[null,"Repair concrete surface with SIKA monotop 615 on SIKA monotop primer, then seal with SIKAFLEX, as per Repair concrete surface with SIKA monotop 615 on SIKA monotop primer, then seal with SIKAFLEX, as per manufacture's specification","m2",230]
[]
[null,"MAKING GOOD OF FINISHES, ETC"]
[null,"Making good"]
[null,"Make good screed to floors to receive new floor\ncoverings (elsewhere) ","m2",230]
[]
[null,"SECTION NO.8 BLOCK H - 4 CLASSROOMS"]
[null,"BILL NO.2"]
[null,"ROOF COVERINGS, ETC."]
[null,"PREAMBLES"]
[]
[null,"The  tenderer  is  referred  to  the  relevant  clauses  in  the separate document Model Preambles for Trades  (2017 Edition) and to the Supplementary Preambles which are incorporated in this Bill."]
[]
[null,"SERVICE, REPAIRS, ETC. TO EXISTING"]
[null,"WORKS"]
[]
[null,"Service, repair and make good existing roof coverings"]
[]
[null,"Service  and  make  good  the  existing  roof  coverings including   refixing   roof   sheets   with   new   galvanised screws, patching all roof leaks with derbigum and leave roof  in  fully  functional  state  for  end  user.  (Provisional)\n(All leaking roofs iBlocks B, C and D","m2",230]
[]
[null,"SECTION NO.8 BLOCK H - 4 CLASSROOMS"]
[null,"BILL NO.3"]
[null,"CARPENTRY AND JOINERY"]
[null,"PREAMBLES"]
[null,"The  tenderer  is  referred  to  the  relevant  clauses  in  the separate  document  Model  Preambles  for  Trades  (2017 Edition) and to the Supplementary Preambles which are incorporated in this Bill."]
[]
[null,"Fixing:\nItems  described  as  nailed  shall  be  deemed  to be  fixed with  hardened  stainless  steel  nails/slots  pins/spinless screws to brick or concrete.\nFixing brackets to be hot dipped galvanised where items not specifically mentioned.\nItems   described   as   \"plugged\"   shall   be   deemed   to include  screwing  to  fibre,  plastic  or  metal  plugs  at  not exceeding  500mm  centres,  and  where  described  as \"bolted\", the bolts have been given elsewhere\nDecorative thermosetting plastic laminate covering"]
[]
[null,"Laminate  covering  shall  be  glued  under  pressure  and edge  strips  of  same  shall  be  butt  jointed  at  junctions with adjacent similar finish"]
[]
[null,"EAVES, VERGES, ETC"]
[null,"'Everite Nutech'' Medium density fibre-cement facia board with H-profile plastic fascia jointers"]
[null,"12  x  225mm  Fascia  boards,  including  aluminium  H- profile   fascia   joiners    and   fixed   with   hot    dipped galvanised drive screws and washers (no paint) (Everite\nNutech - product number 041-203 and 685-195)","m",61]
[]
[null,"''Everite Nutech'' Fibre-cement socketless barge boards"]
[null,"10 x 80 x 225mm Barge boards including aluminium H- profile    barge    joiners    and   fixed    with    hot    dipped galvanised drive screws and washers (no paint) (Everite Nutech - product number 721-800)","m",18]
[]
[null,"DOORS, ETC."]
[null,"Refer to Architectural door schedule. \"Saligna Blaco\""]
[null,"40mm  Framed  ledged  and  braced  batten  door  813  x 2032mm high with 40 x 110mm styles and top rail, 20 x 150mm middle ledge, 20 x 225mm bottom ledge and 20 x 110mm braces filled in with V-jointed one side vertical boarding with tongued and grooved joints to top rail and stiles and with inner edges of framing and abutting edges of boarding chamfered to form V-joint (D1)","No",2]
[]
[null,"SKIRTINGS"]
[null,"Wrought meranti"]
[null,"19 x 76mm Skirtings with 19mm quadrant bead, plugged ","m",121]
[]
[null,"SECTION NO.8 BLOCK H - 4 CLASSROOMS"]
[null,"BILL NO.4"]
[null,"CEILINGS, PARTITIONS AND ACCESS FLOORING"]
[null,"PREAMBLES"]
[null,"The  tenderer  is  referred  to  the  relevant  clauses  in  the separate  document  Model  Preambles  for  Trades  (2017 Edition) and to the Supplementary Preambles which are incorporated in this Bill.\n_\nSUPPLEMENTARY PREAMBLES"]
[]
[null,"Fixing\nItems described as \"nailed\" shall be deemed to be fixed with hardened steel nails  or pins, or to be shot-pinned, to brickwork or concrete\nItems   described   as   \"plugged\"   shall   be   deemed   to include  screwing  to  fibre,  plastic  or  metal  plugs  at  not exceeding  500mm  centres,  and  where  described  as \"bolted\", the bolts have been given elsewhere\nCeilings"]
[]
[null,"Unless otherwise described ceilings shall be deemed to be horizontal"]
[]
[null,"CEILINGS, ETC."]
[null,"NAILED-UP CEILINGS"]
[]
[null,"6.5mm Gypsum plasterboard with H-profile metal steel jointing strips"]
[null,"Ceilings including 50 x 50mm sawn softwood brandering at  400mm  centres  generally  in  one  direction  and  50  x 50mm branders and cross branders at joints and edges","m2",230]
[null,"of boards"]
[]
[null,"Extra  over  ceiling  for  600  x  600mm  trap  door  of  38  x 114mm   softwood   rebated   framing   with   one   cross brander,  covered  with  ceiling  board  and  fitted  flush  in\nopening, including necessary trimmers around","No",2]
[]
[null,"\"Rhino\" gypsum plasterboard cornices"]
[null,"5mm Coved cornices ","m",121]
[]
[null,"\"Isotherm\" insulation\n"]
[null,"50mm   Insulation   closely  fitted   and   laid   on   top   of brandering between roof timbers, etc ","m2",230]
[]
[null,"SECTION NO.8 BLOCK H - 4 CLASSROOMS"]
[null,"BILL NO.5"]
[null,"FLOOR COVERINGS, PLASTIC LININGS, ETC."]
[null,"PREAMBLES"]
[null,"The  tenderer  is  referred  to  the  relevant  clauses  in  the separate  document  Model  Preambles  for  Trades  (2017 Edition) and to the Supplementary Preambles which are incorporated in this Bill."]
[]
[null,"SUPPLEMENTARY PREAMBLES"]
[null,"Fixing"]
[null,"Floor coverings, wall linings, etc shall, where applicable, be   fixed   with   adhesive   as   recommended   by   the manufacturers of the flooring, linings, etc"]
[]
[null,"FLOOR COVERINGS"]
[null,"VINYL FLOOR COVERINGS"]
[]
[null,"2mm thick x 1200mm wide Superflex fully flexible vinyl floor tiles","m2",230]
[null,"On floors"]
[]
[null,"POLISH, SEALERS, ETC"]
[null,"Three coats waterbased sealer on vinyl flooring.","m2",230]
[]
[null,"SECTION NO.8 BLOCK H - 4 CLASSROOMS"]
[null,"BILL NO.6"]
[null,"IRONMONGERY"]
[null,"PREAMBLES"]
[null,"The  tenderer  is  referred  to  the  relevant  clauses  in  the separate document Model Preambles for Trades  (2017 Edition) and to the Supplementary Preambles which are incorporated in this Bill."]
[]
[]
[null,"LOCKS"]
[null,"\"Dorma\" or similar approved"]
[null,"\"Ref 390/313\" four-lever mortice lockset","No",2]
[]
[null,"SUNDRIES"]
[null,"38mm Diameter rubber door stop plugged","No",2]
[]
[null,"KEY TAGS"]
[null,"28mm  Diameter  x  1mm  thick  brass  key  tags  with  one numeral and one letter engraved","No",2]
[]
[null,"Approved standard stainless steel key rings","No",2]
[]
[null,"WRITING BOARDS, ETC"]
[null," \"Parrot\" or equal approved"]
[null,"Model  2203  white  vitreous   enamelled  wall  mounted white   board   2400   x   900mm   high   complete   with aluminium pen rail etc fixed to brickwork or partition system ( Magnetic)","No",4]
[]
[null,"EP09  Floortime domestic  pinning  boards  fixed  to brickwall strictly  in  accordance  to  manufacturer's instructions"]
[null,"2400 x 1200mm high pinning board fixed 900mm above finished floor level","No",4]
[]
[null,"Green   chalkboard  to   comply   with   CKS-38-1980 complete with chalk rail fixed in accordance with the manufacturers specifications","No",4]
[]
[]
[null,"SECTION NO.8 BLOCK H - 4 CLASSROOMS"]
[null,"GRADE R BLOCK"]
[null,"PREAMBLES\nThe tenderer is referred to the relevant clauses in the\nseparate document Model Preambles for Trades (2017\nEdition) and to the Supplementary Preambles which are\nincorporated in this Bill."]
[]
[null,"PLUMBING AND DRAINAGE (PROVISIONAL)"]
[]
[null,"RAINWATER DISPOSAL"]
[null,"0.6mm Chromadek seamless gutters and rainwater pipes"]
[]
[null,"155 x 100 x 115mm aluminium ogee roof gutters with baked enamel finish fixed with concealed brackets","m",61]
[]
[null,"Extra over gutter for stopped end","No",4]
[]
[null,"75 x 100mm Diameter rainwater pipes","m",16]
[]
[null,"Extra over gutter for outlet for 100 x 75mm pipe","No",6]
[]
[null,"Extra over 100mm rainwater pipe for eaves or plinth offset 650mm projection.","No",6]
[]
[null,"FIRE APPLAINCES, ETC"]
[null,"\"Chubb\" or other equal and approved fire\nappliances all to SABS 543 requirements"]
[]
[null,"4.5kg Dry chemical powder portable fire extinguisher","no",2]
[]
[null,"190 x 190mm ABS plastic symbolic safety sign type FB2 plugged and screwed to wall.","no",2]
[]
[]
[null,"SECTION NO.8 BLOCK H - 4 CLASSROOMS"]
[]
[null,"BILL NO.8\nGLAZING\nPREAMBLES\nThe tenderer is referred to the relevant clauses in the separate document Model Preambles for Trades (2017 Edition) and to the Supple"]
[]
[null,"GLAZING TO STEEL WITH PUTTY"]
[null,"6mm Clear float glass\n\nPanes exceeding 0,1m2 and not exceeding 0,5m2","m2",26]
[]
[null,"SECTION NO.8 BLOCK H - 4 CLASSROOMS"]
[]
[null,"BILL NO.9"]
[]
[null,"PAINTWORK"]
[null,"\nThe tenderer is referred to the relevant clauses in the separate document Model Preambles for Trades (2017 Edition) and to the Supplementary Preambles which are incorporated in this Bill."]
[]
[null,"SUPPLEMENTARY PREAMBLES\nPAINT SPECIFICATIONS\nAll painting shall be done in accordance with \"Plascon\" specifications unless otherwise described\nPrime all skirtings and timber work not visible prior to installation. Further paint all glazing beads and reveals prior to glazing.\nPrimers and first coats may be thinned in accordance with the paint specifications to aid the absorption of the paint.\nWhere surfaces of plaster etc are sandy / friable, the first coat must be replaced with 'Merit' plaster primer thinned 10% with turpentine.\nAll surfaces must be sound, clean and have a moisture content of less than 8% for walls generally and 3% for slabs/screeds etc.\nThe paint and surface finishes specified herein are for normal applications as intended by the manufacturer. Should a finish be required for a surface other than that for which it would normally be used, then the specifier should contact manufacturer for approval."]
[]
[null,"COLOURS\nUnless otherwise described all paintwork shall be deemed to have a colour value in excess of 7 on the Munsell system in accordance with SANS 1091"]
[]
[null,"PAINTWORK ETC."]
[null,"ON INTERNAL FLOATED PLASTER SURFACES\nPrepare surfaces and remove all loose material, apply one coat 'Plascon Wall and All Pure Acrylic' thinned 20% and one coat 'Plascon Wall and All Pure Acrylic' paint or equal and approved:"]
[]
[null,"On internal walls.","m2",322]
[]
[null,"External walls","m2",205]
[]
[]
[null,"ON WOOD"]
[null,"Stop, sand down and prepare wood surfaces and apply one coat wood primer, one undercoat and two coats high gloss enamel paint:"]
[]
[null,"On doors","m2",13]
[]
[null,"ON FIBRE-CEMENT"]
[null,"Apply Plascon meit plaster primer and two coats Plascon Velvaglo Polyurethane Enamel paint."]
[]
[null,"Fascias and barge boards.","m",79]
[]
["SECTION SUMMARY - BLOCK G GRADE R BLOCK"]
[]
[null,"Alterations and Demolitions",117]
[]
[null,"Roof Coverings",118]
[]
[null,"Carpentry and Joinery",120]
[]
[null,"Ceilings, Partitions and Access Flooring",122]
[]
[null,"Floor Coverings",123]
[]
[null,"Ironmonery",125]
[]
[null,"Plumbing and Drainage",126]
[]
[null,"Glazing",127]
[]
[null,"Paintork",129]
[]
[]
[null,"SECTION NO.8"]
[null,"BILL NO. 1"]
[]
[null,"BLOCK I - MOBILE CLASSROOM"]
[null,"SUPPLY OF MOBILE CLASSROOM"]
[null,"Allow for the sum of R250,000.00 (Two Hundred and Fifty Thousand) for design, supply and fix to position the mobile classroom","item",250000,250000]
[]
[null,"Profit","%"]
[]
[null,"Attendance","%"]
[]
[null,"Transportation"]
[null,"Allow for the sum of R20,000.00 (Twenty Thousand Rands) for transportation of the mobile unit","item",20000,20000]
[]
[null,"Profit","%"]
[]
[null,"Attendance","%"]
[]
[null,"SECTION NO.9"]
[null,"ELECTRICAL WORKS"]
[]
[null,"BILL NO.1"]
[null,"Preliminary & General\nThe Contractor shall at his own cost, supply all samples that may be required. Material or work not conforming to the approved samples shall be rejected. The Engineer reserves to himself the right to submit samples to any tests to ensure that the material represented by the sample conforms to the requirements of the specifications."]
[]
[null,"Amount required to comply with the Conditions of Contract","SUM"]
[]
[null,"Amount required to comply with the Technical Specification","SUM"]
[]
[null,"Amount required to comply with Health & Safety Specification","SUM"]
[]
[null,"Site Establishment"]
[]
[null,"Amount required as a Fixed Amount","SUM"]
[]
[null,"Amount required as Adjustable with Contract Period","SUM"]
[]
[null,"Amount required as Adjustable with Contract Amount","SUM"]
[]
[null,"SECTION NO.9"]
[null,"ELECTRICAL WORKS"]
[]
[null,"BILL NO. 2"]
[null,"LV RETICULATION"]
[]
[null,"Refurbishment of Main DB and issuing of COC","SUM"]
[]
[null,"Refurbishment and modification of DB-1 and issuing of COC","SUM"]
[]
[null,"Refurbishment and modification of DB-2 and issuing of COC","SUM"]
[]
[null,"Refurbishment and modification of DB-3 and issuing of COC","SUM"]
[]
[null,"Refurbishment and modification of DB-4 and issuing of COC","SUM"]
[]
[null,"Refurbishment and modification of DB-5 and issuing of COC","SUM"]
[]
[null,"Supply and Installation of 1 x 35mm2 4C PVC/SWA/Cu cable","m",50]
[]
[null,"Supply and Installation of 1 x 25mm2 BCEW","m",50]
[]
[null,"Cable terminations for 1 x 35mm2 4C PVC/SWA/Cu cable to new Prefab cLassrooms","m",6]
[]
[null,"Earth terminations for 1 x 25mm2 BCEW","m",6]
[]
[null,"Electrical wireways: P8000 trunking complete covers, bends and accessories","m",500]
[]
[null,"Sleeves wireways: 50mm diameter HDPE","m",100]
[]
[null,"SECTION NO.9"]
[null,"ELECTRICAL WORKS"]
[null,"BILL NO. 3"]
[null,"POWER INSTALLATION"]
[null,"Supply, installation and Wiring of 16A Switched Socket outlet (SANS 164-1, 164-2) c/w 4mm2 L+N & 2.5mm2 E copper conductors wired from DB.","No",28]
[]
[null,"Allow for an electrical heating system / air-conditioners, 32A Isolators for heaters / aircon c/w 6mm2 L+N & 4mm2 E copper conductors wired from DB, 3 phase cable to DB and additional circuit breakers per\nclassroom","No",12]
[]
[null,"SECTION NO.9"]
[null,"ELECTRICAL WORKS"]
[]
[null,"BILL NO. 4"]
[null,"LIGHTING INSTALLATION"]
[]
[null,"Supply and installation of Type A Luminaire: 2 x 18W Linear LED Vapourproof (T8) 1500mm long, mild steel, c/w accessories (min. efficacy: 105 lm/W)","SUM"]
[]
[null,"5A unswitched sockets for Type A Luminaire c/w\n2.5mm2 L+N & 1.5mm2 E copper conductors wired from DB.","SUM"]
[]
[null,"Supply and installation of Type C Luminaire: Round\nBulkhead c/w 2x9W E27 LED Lamps, Surface mounted, die cast aluminium body and polycarbonate diffuser.","SUM"]
[]
[null,"Control point for Type C Luminaire c/w 2.5mm2 L+N & 1.5mm2 E copper conductors wired from DB.","SUM"]
[]
[null,"Supply and installation of Type VP Luminaire: Round Bulkhead c/w 2x9W E27 LED Lamps, Surface mounted, die cast aluminium body and polycarbonate diffuser.","SUM"]
[]
[null,"Control point for Type VP Luminaire c/w 2.5mm2 L+N & 1.5mm2 E copper conductors wired from DB.","SUM"]
[]
[null,"Supply and install light switch c/w 2.5mm2 L+N & 1.5mm2 E copper conductors wired from DB.","SUM"]
[]
[null,"Supply and install 16A Day/night switch, IP65 installed in empty rectangular bulkhead fitting","SUM"]
[]
[null,"SECTION NO.9"]
[null,"ELECTRICAL WORKS"]
[null,"BILL NO. 5"]
[]
[null,"EARTHING AND LIGHTNING PROTECTION INSTALLATION"]
[]
[null,"PC SUMS for installation of Earthing and Lightning Protection as per the design and issuing of Certificate of Compliance.","SUM"]
[]
["SECTION SUMMARY - ELECTRICAL WORKS"]
[]
[null,"Preliminaries",132]
[]
[null,"LV Reticulation",133]
[]
[null,"Power Installation",134]
[]
[null,"Lighting Installation",135]
[]
[null,"Earthing and lightening Protection Installation",136]
[]
[null,"SECTION NO.10"]
[null,"CIVIL WORKS"]
[null,"BILL NO.1"]
[]
[null,"WATER RETICULATION"]
[]
[null,"Total length of pipe to be constructed, 160 mm Ø HDPE class 12","m",110]
[]
[null,"Total length of pipe to be constructed, 90 mm Ø HDPE class 12","m",130]
[]
[null,"Excavations over 1,0 m but not exceeding 2,5 m","m",240]
[]
[null,"Excavation 90mm HDPE class 12"]
[null,"Bedding","m3",8]
[]
[null,"Selected backfill","m3",4]
[]
[null,"General Backfill","m",54]
[]
[null,"Excavation 160mm HDPE class 12"]
[null,"Bedding","m3",8]
[]
[null,"Selected backfill","m",8]
[]
[null,"General Backfill","m3",50]
[]
[null,"Water fittings as required and specified (valves, etc)","item",1]
[]
[null,"Pressure testing of existing pipe network","item",1]
[]
[null,"Storage tank including all fittings and infrastructure","item",1]
[]
[null,"SECTION NO.10"]
[null,"CIVIL WORKS"]
[]
[null,"BILL NO. 2"]
[null,"STORMWATER"]
[]
[null,"Demolishing and removal of existing damaged V-drains","m",350]
[]
[null,"Reinforced concrete 25mpa/19mm stone in new stormwater V-drains","m",350]
[]
[null,"Ref 193 mesh reinforcement","m2",350]
[]
["SECTION SUMMARY - CIVIL WORKS"]
[]
[null,"Water Reticulation",138]
[]
[null,"Stormwater",139]
[]
[null,"SECTION NO.11"]
[null,"EXTERNAL WORKS"]
[]
[null,"BILL NO. 1"]
[null,"GENERAL SITE WORKS"]
[null,"PREAMBLES"]
[null,"The tenderer is referred to the relevant clauses in the\nseparate document Model Preambles for Trades (2009\nEdition) and to the Supplementary Preambles which are\nincorporated in this Bill"]
[]
[null,"WATER TROUGH"]
[null,"Allow for Water trough revamp as per architectural instructions complete","item",1]
[]
[null,"PLAYING STRUCTURES"]
[null,"Allow for supply, prepare, and construction of Slide\ncomplete according to Architect specifications and requirements. (Refer to specifications Document)","item",1]
[]
[null,"Allow for supply, prepare, and construction of Climbing Ladder complete according toArchitect specifications and requirements. (Refer to specifications Document)","No",2]
[]
[]
[null,"Allow for supply, prepare, and construction of Swings complete according toArchitect specifications and requirements. (Refer to specifications Document)","No",2]
[]
[]
[null,"Prepare and build square shaped sand pit size 4000 x 4000mm complete as per the architectural drawings","item",1]
[]
[null,"CONCRETE"]
[null,"Concrete small works"]
[]
[null,"220 x 100mm Thick triangular edging to paving including excavations etc","m",100]
[]
[null,"PRECAST CONCRETE PAVING BLOCKS\nPaving is to be laid in accordance with SABS 1200MJ, SABS 1058 and the Concrete Masonry Association's Specification\nStandard \"Grey\" or similar approved interlocking roadstone paving on and including 25mm thick layer of river sand with joints filled in with sand, compacted with a vibration roller"]
[]
[null,"80mm Paving to extending assembly area, walkways,\netc. to falls","m2",400]
[]
[null,"PRECAST KERBS"]
[null,"Precast concrete barrier kerb fig.12 edge restraint, bedded, jointed and pointed in 1-3 cement mortar including shallow excavation, small concrete foundation and concrete benching behind joints.","m2",150]
[]
[null,"ALUMINIUM FLAGPOLE"]
[null,"The following in a 8,5m high standard government type aluminium flagpole as \"Aluweld\" or other similar approved and erected on 600 x 600 x 800mm deep 20Mpa concrete base, including excavations, carting away, etc."]
[]
[null,"Aluweld\" or similar approved aluminium flagpole comprising 76mm and 50mm outside diameter aluminium tubing tapered by way of an aluminium cone casting, welded, and complete with spherical top cap, two pulleys, two cleats, two halyards (ropes) and swivel\ntype base, etc.","no",1]
[]
[null,"PLAY GROUNDS"]
[null,"Allow for levelling of play grounds as directed by the Engineer complete","item",1]
[]
[null,"Extra over all excavations for carting away"]
[null,"Surplus material from excavations and/or stock piles on site to a dumping site to be located by the contractor.","m3",250]
[]
[null,"STRUCTURAL STEEL REPAIRS"]
[null,"Allow for the repairs of damaged structural steel structures on site, supply and replace where necessary make good and paint as directed by the Engineer and the Architect.","t",6.2]
[]
[null,"Allow for supply and fit new structural steel parts (Remeasurable on site)","t",5]
[]
[null,"Allow for all necessary accessories to complete the above","item",1]
[]
[null,"SECTION NO.11"]
[null,"EXTERNAL WORKS"]
[]
[null,"BILL NO. 2"]
[null,"DEMOLITION WORKS"]
[null,"PREAMBLES\nThe tenderer is referred to the relevant clauses in the\nseparate document Model Preambles for Trades (2017\nEdition) and to the Supplementary Preambles which are\nincorporated in this Bill"]
[]
[null,"DEMOLITIONS"]
[null,"Removal of Mobile Classrooms"]
[null,"Removal of mobile classroom size 6000mm x 9000mm\nlong x 2650mm high including transportation and cartaway","no",1]
[]
[null,"Demolitions"]
[null,"Breakup and demolish the existing concrete surface bed\noverall size 4069 x 4594mm long, cart away the rubble\nand unwanted materials to an authorised place, prepare the area to receive new platform.","m",1]
[]
[null,"Breakup and demolish the existing concrete surface bed\noverall size 3648 x 6255mm long, cart away the rubble\nand unwanted materials to an authorised place, prepare the area to receive new platform.","no",1]
[]
[null,"Allow for demolishing complete approximate overall size\n3678 x 6255mm long, levelling and cart away of\nunwanted materials to an authorised municipal place, the existing concrete surface bed","no",1]
[]
[null,"Allow for demolishing complete approximate overall size\n3678 x 4594mm long, levelling and cart away of\nunwanted materials to an authorised municipal place, the existing concrete surface bed..","no",1]
[]
[null,"ASBESTOS REMOVAL"]
[null,"Allow for removal of asbestos by the specialists, loading, dumping to the authorised municipal site, provide the specialist details with the tender.","item",1]
[]
[null,"Allow for testing the roof materials suspected to be Asbestos before removal","item",1]
[]
[null,"SECTION NO.11"]
[null,"EXTERNAL WORKS"]
[]
[null,"BILL NO.2"]
[null,"FENCING AND GATES"]
[]
[null,"PREAMBLES\nThe tenderer is referred to the relevant clauses in the\nseparate document Model Preambles for Trades (2008\nEdition) and to the Supplementary Preambles which are\nincorporated in this Bill"]
[]
[null,"REMOVAL OF EXISTING FENCE"]
[null,"Break down and remove existing fence and gate\ncomplete with all posts, droppers, concrete footings, concrete underdig, etc.","m",448]
[]
[null,"SECURITY FENCING"]
[null,"THE FOLLOWING WORK SHALL BE UNDERTAKEN\nBY REPUTABLE CONTRACTORS WHO ARE TO BE\nAPPROVED BY THE PRINCIPAL AGENT PRIOR TO\nCOMMENCING ANY WORK ON SITE"]
[]
[null,"ClearVu or equal approved fencing"]
[]
[null,"ClearVU or equal approved anti-climbing and anti- cut pressed mesh panel fencing 2,1m high, formed of 3mm dia. horizontal and 4mm dia. vertical high tensile line galvanised with polymer coating wires with aperture size 76,2mm x 12,7mm and reinforcing V-section ribs, bolted with vandal resistant bolts and clamping plates to 60 x 60 x 3mm square tube posts 2,75m high at 2,534m centres with sealed end caps and 30 x 3mm x 250mm long angle section base anchors with posts bedded in 15MPa concrete bases size 400 x 400 x 600mm deep with anti theft double bar riveted to mesh and mesh base:"]
[]
[null,"1800mm High fencing","m",448]
[]
[null,"100mm high powder coated charcoal shark tooth type spike rail, bolted to 50mm wide mesh fencing flange bent along the top","m",448]
[]
[null,"200 x 200mm concrete sill for anti-burrow including excavations, cartaway, backfilling, formwork to sides, etc.","m",448]
[]
[null,"Extra over fencing for all necessary accessories, components, transportation, etc.","item",1]
[]
[null,"GATES"]
[null,"Purpose made sliding gate size 7000 x 2100mm high\ncomplete with, rail, motor, lock and locking mechanism","no",1,null,{"$f":"+F2296:F2299","v":0}]
[]
[null,"Purpose made pedestrian gate size 1000 x 2100mm high complete with lock and locking mechanism","no",2]
[]
["SECTION SUMMARY - EXTERNAL WORKS"]
[]
[null,"General External Works",143]
[]
[null,"Demolitions",145]
[]
[null,"Fencing",147]
[]
[]
[null,"CPD BUILD PROGRAMME"]
[]
[null,"Note to tenderers: As CPGs may not provide any bidder a competitive advantage. Provisional amounts and fixed percentages for profit and attendance have been provided. Only the provisional amount will be adjusted once the awarded tender amount and/or the beneficiaries have been appointed, and the final values have been ascertained. "]
[]
[null,"MINIMUM TARGETED LOCAL BUILDING MATERIAL MANUFACTURERS"]
[null,"Provision is made for the Minimum Targeted Local Building Material Manufacturers CPG in the execution of this project as described in   C3.1 Project Specifications.  Allowance for monitoring and monthly reporting on material purchased from Local Building Material Manufacturers by main contractor and subcontractors based on determination by Employer taking into account specific project variables","PS",1,{"v":23588.77695,"d":"23,588.78"},{"$f":"E2317","v":{"v":23588.77695,"d":"23,588.78"}}]
[null,"Allowance for profit and attendance, all inclusive of associated costs to the contractor for implementation. ","%"]
[]
[null,"Allowance for attendance all inclusive of associated costs to the contractor for implementation. ","%"]
[]
[null,"MINIMUM TARGETED LOCAL BUILDING MATERIAL SUPPLIERS "]
[null,"Provision is made for the Minimum Targeted Local Building Material Suppliers CPG in the execution of this project as described in   C3.1 Project Specifications. Allowance for monitoring and monthly reporting on material purchased from Local Building Material Suppliers by main contractor and subcontractors based on determination by Employer  taking into account specific project variables ","PS",1,{"v":23588.77695,"d":"23,588.78"},{"$f":"E2323","v":{"v":23588.77695,"d":"23,588.78"}}]
[null,"Allowance for profit all inclusive of associated costs to the contractor for implementation. ","%"]
[null,"Allowance for attendance all inclusive of associated costs to the contractor for implementation. ","%"]
[]
[null,"MINIMUM TARGETED ENTERPRISE DEVELOPMENT"]
[null,"A provisional amount has been allowed for in the execution of this project as described in  C3.1 Project Specifications. The provisional amount allowed is for the appointment of training coordinator, mentor, training service providers and training of the beneficiary enterprises including monitoring and monthly reporting.","PS",1,235887.7695,{"$f":"E2328","v":{"v":235887.7695,"d":"235,887.77"}}]
[null,"Allowance for profit all inclusive of associated costs to the contractor for implementation. ","%"]
[null,"Allowance for attendance all inclusive of associated costs to the contractor for implementation. ","%"]
[]
[null,"LABOUR INTENSIVE PARTICIPATION GOAL"]
[null,"Labour Intensive Participation Goal - Allowance for monthly reporting of labour intensive works by main contractor based on determination by Employer taking into account specific project variables. Allowance for monitoring and monthly reporting on Works executed by means of Labour Intensive methods by main contractor and subcontractors based on determination by Employer taking into account specific project variables ",null,1,72000,{"$f":"E2333","v":{"v":72000,"d":"72,000.00"}}]
[null,"Allowance for profit all inclusive of associated costs to the contractor for implementation. ","%"]
[null,"Allowance for attendance all inclusive of associated costs to the contractor for implementation. ","%"]
[]
[null,"APPOINTMENT OF CLO",null,"H3",0]
[]
[null,"Make alllowance of R100 000.00 for appointment of CLO for the project duration of 10 months",null,"Item",1,{"v":100000,"d":"100,000.00"}]
[]
[]
[null,"PRELIMINARIES","Page",24]
[]
[null,"BLOCK A - GUARD HOUSE","Page",45]
[]
[null,"BLOCK B , C AND D - ABLUTION BLOCKS","Page",57]
[]
[null,"BLOCK E - 4 CLASSROOM BLOCK, ADMIN OFFICE AND STUFF ROOM OFFICE","Page",78]
[]
[null,"BLOCK F - SNP KITCHEN","Page",96]
[]
[null,"BLOCK G - GRADE R BLOCK","Page",114]
[]
[null,"BLOCK H - 4 CLASSROOMS","Page",130]
[]
[null,"BLOCK I - MOBILE CLASSROOM","Page",131]
[]
[null,"ELECTRICAL WORKS","Page",137]
[]
[null,"CIVIL WORKS","Page",140]
[]
[null,"EXTERNAL WORKS","Page",148]
[]
[null,"PROVISION AL SUMS","Page",150]
[]
[null,"SUB-TOTAL","ST"]
[]
[null,"CONTINGENCIES"]
[]
[null,"Allow Five per cent (5%) of the above sub-total for contingencies to be used as directed and deducted in whole or in part if not required.","TAX",5]
[]
[null,"SUB-TOTAL:","ST"]
[]
[null,"Add Value Added Tax at the rate of 15%","TAX",15]