{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Dr Blok"],"not_rendered":{"external_links":1,"defined_names":6},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Dr Blok","index":0,"n_rows":153,"n_cols":7,"rows_kept":153,"merged":[[0,0,1,6],[2,0,3,6],[5,0,5,6],[152,1,152,5]],"flags":["formulas_cached_only"]}
["DR. BLOK SECONDARY SCHOOL"]
[]
["ELECTRICAL BILL OF QUANTITIES"]
[]
[]
["DEVELOPMENT BANK OF SOUTHERN AFRICA"]
[]
["Item No","Description",null,"Quantity","Rate","Rate","Amount"]
[]
[null,"Lighting and Small Power"]
[]
[1,"400V kiosk"]
[]
[1.1,"Decommission, Disconnect, Mark all cables, Remove and Store old uncompliate Kiosks","No",1,null,null,0]
[]
[1.2,"Supply, manufacture, deliver, install 400V and commission new Kiosk complete with all accessories as per the drawings","No",3,null,null,0]
[]
[2,"SUB-DISTRIBUTION BOARD 400V 5KA"]
[]
[2.1,"Supply, manufacturer,Install and commission 400V SP&L distribution boad complete with all accessories as per the drawing","No",17,null,null,0]
[]
[3,"LIGHT FITTINGS"]
[3.1,"Suppy, deliver and install the following light fittings complete; inclusive of lamps"]
[]
[3.2,"2X36W 1200mm open channel T5 light fitting ","No",400,null,null,0]
[]
[3.3,"1X22W IP65 Bulkhead light fitting ","No",145,null,null,0]
[]
[3.4,"1X22W IP28 Bulkhead light fitting","No",90,null,null,0]
[]
[4,"LIGHT SWITCHES"]
[]
[4.1,"Supply, install and connect flush mounted switch unit complete with cover plate, boxes and all accessories"]
[]
[4.2,"Single Lever, 1 Way light switch","No",130,null,null,0]
[]
[4.3,"Single Lever, 2 Way light switch","No",0,null,null,0]
[]
[4.4,"Photocell in a blulkhead ","No",17,null,null,0]
[]
[]
[]
[5,"CONDUCTORS AND CABLES"]
[]
[5.1,"Supply and install GP PVC insulated copper conductors in required colours drawn into conduit or in trunking"]
[]
["5.1.2","2,5 mm² ","m",8000,{"v":6.26,"d":"R 6.26"},null,0]
[]
["5.1.3","4 mm² ","m",8000,null,null,0]
[]
[5.2,"Supply, deliver and install  PVC, PVC, SWA, PVC  600/1000V cables"]
[]
["5.2.1","4 mm², 4-Core ","m",60,null,null,0]
[]
["5.2.2","6 mm², 4-Core ","m",100,null,null,0]
[]
["5.2.3","10 mm², 4-Core","m",850,null,null,0]
[]
["5.2.4","16 mm², 4-Core ","m",135,null,null,0]
[]
[]
["5.2.5","25 mm², 4-Core ","m",200,null,null,0]
[]
["5.2.6","70 mm², 4-Core","m",280,null,null,0]
[]
["5.2.7","240 mm², 4-Core","m",70,null,null,0]
[]
[5.3,"Supply, deliver and install single core antitheft copper coated bare earth conductor"]
[]
["5.3.1","4 mm², 1-Core ","m",60,null,null,0]
[]
["5.3.2","6 mm², 1-Core ","m",100,null,null,0]
[]
["5.3.3","10 mm², 1-Core","m",850,null,null,0]
[]
["5.3.4","16 mm², 1-Core ","m",400,null,null,0]
[]
["5.3.5","35 mm², 1-Core ","m",280,null,null,0]
[]
["5.3.6","120 mm², 1-Core ","m",70,null,null,0]
[]
[6,"Cable Termination"]
[]
[6.1,"supply, deliver and install termination kit, complete with compression gland, lugs, sleeves and all accessories"]
[]
["6.1.1","240 mm², 4-Core PVC, PVC, SWA, PVC  600/1000V cable","No",2,null,null,0]
[]
["6.1.2","70 mm², 4-Core PVC, PVC, SWA, PVC  600/1000V cable","No",4,null,null,0]
[]
["6.1.3","25 mm², 4-Core PVC, PVC, SWA, PVC  600/1000V cable","No",2,null,null,0]
[]
["6.1.4","16 mm², 4-Core PVC, PVC, SWA, PVC  600/1000V cable","No",2,null,null,0]
[]
["6.1.5","10 mm², 4-Core PVC, PVC, SWA, PVC  600/1000V cable","No",26,null,null,0]
[]
["6.1.6","6 mm², 4-Core PVC, PVC, SWA, PVC  600/1000V cable","No",4,null,null,0]
[]
["6.1.7","4 mm², 4-Core PVC, PVC, SWA, PVC  600/1000V cable","No",2,null,null,0]
[]
["6.1.8","2,5mm² GP PVC insulated copper conductors","No",110,null,null,0]
[]
["6.1.9","4 mm² GP PVC insulated copper conductors","No",190,null,null,0]
[]
["6.1.10","4 mm² single core antitheft copper coated bare earth conductor","No",1,null,null,0]
[]
["6.1.11","6 mm² single core antitheft copper coated bare earth conductor","No",2,null,null,0]
[]
["6.1.12","10 mm² single core antitheft copper coated bare earth conductor","No",13,null,null,0]
[]
["6.1.13","16 mm² single core antitheft copper coated bare earth conductor","No",2,null,null,0]
[]
["6.1.14","35 mm² single core antitheft copper coated bare earth conductor","No",2,null,null,0]
[]
["6.1.15","120 mm² single core antitheft copper coated bare earth conductor","No",1,null,null,0]
[]
[7,"SWITCHED SOCKET OUTLETS and Isolators"]
[]
[7.1,"Supply, install and connect flush mounted switch socket outlets and isolators as specified including cover plates and all accessories"]
[]
["7.1.1","45A wall mounted isolator ","No",0,{"v":103.3,"d":"R 103.30"},null,0]
[]
["7.1.2","16 Amp, 3-pin, double switched socket outlet","No",135,{"v":165.85,"d":"R 165.85"},null,0]
[]
["7.1.3","16 Amp, 3-pin, single switched socket outlet","No",0,null,null,0]
[]
[8,"Conduit and Conduit Boxes"]
[]
[null,"Supply and install 25mm PVC conduit complete with all accessories including adpters and couplers","No",4000,null,null,0]
[]
["6.1","'Supply and install 60 mm round, 60 mm deep PVC box for 20 mm conduit fixed in sofit or brickwork or ceiling void","No",450,{"v":4,"d":"R 4.00"},null,0]
[]
["6.2","Supply and install 100 x 50 x 50 mm galv. box, flush mounted in brickwork","No",90,{"v":9,"d":"R 9.00"},null,0]
[]
["6.3","'Supply and install 100 x 100 x 50 mm galv. box, flush mounted in brickwork","No",190,{"v":9.8,"d":"R 9.80"},null,0]
[]
[9,"EXCAVATION AND BACKFILLING"]
[]
[9.1,"Excavate 800mm deep by 500mm wide hand pickable soil","m",2350,null,null,0]
[]
["9.2","Backfilling","m",2350,null,null,0]
[]
[]
[10,"EARTHING AND BONDING"]
[]
["10.1","Perform soil resistivity test","No",1,null,null,0]
[]
["10.2","Earth and Bond of the complete installation in accordance with the Specifications and SANS Standards.","Sum",1,{"v":3000,"d":"R 3,000.00"},null,0]
[]
[11,"TEST AND COMMISIONING"]
[]
["11.1","Test and Commision the complete installation in accordance with the Specifications and SANS Standards.","Sum",1,{"v":3000,"d":"R 3,000.00"},null,0]
[]
[null,"SECTION 1 TOTAL SUMMARY (Carried to Part B: Electrical Works on Page 115 of the MAIN BOQ)",{"$nulls":4},0]