{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Limpopo Central Hospital"],"read":"whole","date_system":"1900"}

{"sheet":"Limpopo Central Hospital","index":0,"n_rows":13842,"n_cols":5,"rows_kept":13842}
["DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT"]
["SECTION 1","H2",0]
[]
["BILL NO 1","H2",0]
[]
["PRELIMINARIES","H2"]
[]
["MEANING OF TERMS “TENDER / TENDERER”","H2",0]
[]
["Any reference to the words “Tender\" or \"Tenderer\" herein and/or in any other documentation shall be construed to have the same meaning as the words \"Bid\" or \"Bidder\"",null,0]
[]
["PRELIMINARIES","H2",0]
[]
["The JBCC Preliminaries Code 2103, May 2005 edition for use with the JBCC Principal Building Agreement Edition 4.1 Code 2101, March 2005 is taken to be incorporated herein.  The tenderer is deemed to have referred to these documents for the full intent and meaning of each clause.  These clauses are referred to by number and heading only.  Where standard clauses or options are not applicable to the contract such modifications or corrections as are necessary are given under each relevant clause. Where an item is not relevant to this specific contract such item is marked \"N/A\" signifying \"Not Applicable\".",null,0]
[]
["PRICING OF PRELIMINARIES","H2",0]
[]
["Should Option A, as set out in clause B10.3.1 hereinafter  be used for the adjustment of preliminaries then each item priced is to be allocated to  one or more of the three categories Fixed, Value Related or Time Related and the respective amounts entered in the spaces provided under each item",null,0]
[]
["Items not priced in these Preliminaries shall be deemed to be included elsewhere in these Bills of Quantities.",null,0]
[]
["SECTION A: JBCC PRINCIPAL BUILDING AGREEMENT","H2",0]
[]
["DEFINITIONS","H2",0]
[]
["DEFINITIONS AND INTERPRETATION","H2",0]
[]
["Clause 1.0  Clause 1.0 is amended by the addition of the following:  1.5.7 References to any party to this agreement include its successors or permitted assigns;1.5.8 References to the contractor include the obligations of its personnel;1.5.9 References to “month” shall be to a calendar month;1.5.10 References to any amount shall mean that amount exclusive of VAT, unless the amount expressly includes VAT;1.5.11 References containing terms such as “best endeavours\" when used in connection with an obligation of either party, means taking in good faith and with due diligence all reasonable steps to achieve the objective and to fulfil the obligation at the earliest possible time, including doing all that a reasonable and prudent owner or provider of design and construction services in comparable circumstances would do.1.5.12 If a definition imposes substantive rights and obligations on a party, such rights and obligations shall be given effect to and shall be enforceable, notwithstanding that they are contained in a definition; 1.5.13 Where any word is defined within the context of any particular clause in this agreement, that word, unless it is clear from the clause in question that that word has limited application only to the relevant clause, shall bear the meaning ascribed to it for all purposes in terms of this agreement, notwithstanding that that word has not been defined in clause 1.1;1.5.14  Words defined in this agreement shall bear the same meanings in any annexes or schedules to this agreement unless the annexes or schedules contain their own definitions of such words; 1.5.15 Where any number of days is prescribed, those days shall be reckoned exclusively of the first and inclusively of the last day unless the last day falls on a day that is not a working day, in which event the last day shall be the next succeeding working day;1.5.16 Words and abbreviations that have well known technical or trade meanings are used in the agreement in accordance with such recognized meanings;1.5.17 The rule of construction that if general words or terms are used in association with specific words or terms that are a species of a particular genus or class, the meaning of the general words or terms shall be restricted to that same class shall not apply, and whenever the word \"including\" is used followed by specific examples, such examples shall not be interpreted so as to limit the meaning of any word or term to the same genus or class as the examples given;1.5.18 The rule of construction that the agreement shall be interpreted against or to the disadvantage of the party responsible for the drafting or preparation of this agreement shall not apply.1.10 The copyright in all contract documents, contract drawings and records (irrespective of who prepared any of the aforesaid) related in any manner to the works shall vest in the employer and the contractor shall not furnish any information in connection with the works to any person or organization without the prior written approval of the employer to this effect other than subcontractors appointed for purposes of this agreement. 1.11 Any provision in this agreement that is or may become illegal, invalid or unenforceable in any jurisdiction shall be ineffective to the extent of such prohibition or unenforceability in such jurisdiction and shall be treated as severed from the balance of this agreement in such jurisdiction, without invalidating the remaining provisions of this agreement in such jurisdiction or affecting it in any other jurisdiction","Item",1,null,{"$f":"D28*C28","v":{"v":0,"d":"R0.00"}}]
[{"$nulls":4},{"$f":"D29*C29","v":{"v":0,"d":"R0.00"}}]
["Fixed:____________ Value related:____________ Time related:____________ ",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["OBJECTIVE AND PREPARATION","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["OFFER, ACCEPTANCE AND PERFORMANCE","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 2.0","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["DOCUMENTS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 3.0","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 3.5 no clause",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 3.7 is amended by the addition of the following:",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The contractor shall keep a copy of all drawings, schedules, unpriced bills of quantities/lump sum document, contract instructions, minutes of site and other meetings, health and safety files as specified in the scope of work, risk register, claims and variation order register, labour records and subcontractors contracts on the site to which the employer, principal agent and agents shall have access at all times. The employer has the right to call for such further information from the contractor it deems necessary in the event it carries out any investigation or audit into potential fraud, corruption, fronting, health and safety incidents or verifying information the contractor has to supply to the employer in terms of this agreement. The Contractor shall ensure a similar right for the Employer with its subcontractors.",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 3.10 is amended by replacing the first reference to “principal agent” with the word “employer”",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["DESIGN RESPONSIBILITY","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 4.0","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["EMPLOYER’S AGENTS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 5.0","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SITE REPRESENTATIVE","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 6.0","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related: ____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["COMPLIANCE WITH REGULATIONS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 7.0","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 7.0 is amended by the addition of the following clauses:  7.3 The Occupational Health and Safety Act No. 85 of 1993 and the Construction Regulations 2014 will in all respects be applicable to this contract. All obligations in respect of health and safety requirements of the Contractor are set out in the Scope of Work  7.3.1 Notwithstanding any actions which the employer may take, the contractor accepts sole liability for due compliance with the relevant duties, obligations, prohibitions, arrangements and procedures imposed by the Occupational Health and Safety Act, 1993 (Act 85 of 1993), and all its regulations, including the Construction Regulations, 2014, for which the contractor is liable as mandatory. By entering into this agreement it shall be deemed that the parties have agreed in writing to the above provisions in terms of Section 37 (2) of the Act and will enter into the mandatory agreement as set out in the Scope of Work. This clause will be sufficient to establish the mandatory obligations of the contractor in the event the parties fail to execute the aforesaid mandatory agreement.",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Note: The provisions herein include inter alia, compliance with all the requirements set out in the Construction Regulations, 2014 issued under the Occupational Health and Safety Act, 1993 (Act No 85 of 1993), and in particular with Regulation 7(1)(a) requiring the compilation of a health and safety plan, as well as Regulation 8(1) requiring the appointment of a construction supervisor",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["WORKS RISK","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 8.0","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["INDEMNITIES","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 9.0","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D93*C93","v":{"v":0,"d":"R0.00"}}]
["WORKS INSURANCES","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 10.0","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 10.0 is amended by the addition of the following clauses:",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["10.5  Damage to the Works","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["(a)  Without in any way limiting the contractor’s obligations in terms of the contract, the contractor shall bear the full risk of damage to and/or destruction of the works by whatever cause during construction of the works and hereby indemnifies and holds harmless the employer against any such damage. The contractor shall take such precautions and security measures and other steps for the protection and security of the works as the contractor may deem necessary",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["(b) The contractor shall at all times proceed immediately to remove or dispose of any debris arising from damage to or destruction of the works and to rebuild, restore, replace and/or repair the works",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["(c) The employer shall carry the risk of damage to or destruction of the works and material paid for by the employer that is the result of the excepted risks as set out in 10.6",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["(d)  Where the employer bears the risk in terms of this contract, the contractor shall, if requested to do so, reinstate any damage or destroyed portions of the works and the costs of such reinstatement shall be measured and valued in terms of 32.0 hereof",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["10.6 Injury to Persons or loss of or damage to Properties","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["(a) The contractor shall be liable for and hereby indemnifies the employer against any liability, loss, claim or proceeding whether arising in common law or by statute, consequent upon personal injuries to or the death of any person whomsoever arising out of or in the course of or caused by the execution of the works unless due to any act or negligence of any person for whose actions the employer is legally liable",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["(b) The contractor shall be liable for and hereby indemnifies the employer against any liability, loss, claim or proceeding consequent upon loss of or damage to any moveable or immovable or personal property or property contiguous to the site, whether belonging to or under the control of the employer or any other body or person, arising out of or in the course of or by reason of the execution of the works unless due to any act or negligence of any person for whose actions the employer is legally liable",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["(c) The contractor shall, upon receiving a contract instruction from the principal agent, cause the same to be made good in a perfect and workmanlike manner at his own cost and in default thereof the employer shall be entitled to cause it to be made good and to recover the cost thereof from the contractor or to deduct the same from amounts due to the contractor",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["(d) The contractor shall be responsible for the protection and safety of such portions of the premises placed under his control by the employer for the purpose of executing the works until the issue of the certificate of practical completion",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["(e) Where the execution of the works involves the risk of removal of or interference with support to adjoining properties including land or structures or any structures to be altered or added to, the contractor shall obtain adequate insurance and will remain adequately insured or insured to the specific limit stated in the contract against the death of or injury to persons or damage to such property consequent on such removal or interference with the support until such portion of the works has been completed",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["(f) The contractor shall at all times proceed immediately at his own cost to remove or dispose of any debris and to rebuild, restore, replace and/or repair such property and to execute the works",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["10.7 High risk insurance","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["In the event of the project being executed in a geological area classified as a “High Risk Area”, that is an area which is subject to highly unstable subsurface conditions that might result in catastrophic ground movement evident by sinkhole or doline formation the following will apply:",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["10.7.1 Damage to the works","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The contractor shall, from the commencement date of the works until the date of the certificate of practical completion bear the full risk of and hereby indemnifies and holds harmless the employer against any damage to and/or destruction of the works consequent upon a catastrophic ground movement as mentioned above. The contractor shall take such precautions and security measures and other steps for the protection of the works as he may deem necessary",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["When so instructed to do so by the principal agent, the contractor shall proceed immediately to remove and/or dispose of any debris arising from damage to or destruction of the works and to rebuild, restore, replace and/or repair the works, at the contractor’s own costs",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["10.7.2 Injury to persons or loss of or damage to property","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The contractor shall be liable for and hereby indemnifies and holds harmless the employer against any liability, loss, claim or proceeding arising at any time during the period of the contract whether arising in common law or by statute, consequent upon personal injuries to or the death of any person whomsoever resulting from, arising out of or caused by a catastrophic ground movement as mentioned above",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The contractor shall be liable for and hereby indemnifies the employer against any and all liability, loss, claim or proceeding consequent upon loss of or damage to any moveable or immovable or personal property or property contiguous to the site, whether belonging to or under the control of the employer or any other body or person whomsoever arising out of or caused by a catastrophic ground movement, as mentioned above, which occurred during the period of the contract",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["10.7.3 It is the responsibility of the contractor to ensure that he has adequate insurance to cover his risk and liability as mentioned in 10.7.1 and 10.7.2. Without limiting the contractor’s obligations in terms of the contract, the contractor shall, within twenty-one (21) calendar days of the commencement date but before commencement of the works, submit to the employer proof of such insurance policy, if requested to do so",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["10.7.4 The employer shall be entitled to recover any and all losses and/or damages of whatever nature suffered or incurred consequent upon the contractor’s default of his obligations as set out in 10.7.1; 10.7.2 and 10.7.3. Such losses or damages may be recovered from the contractor or by deducting the same from any amounts still due under this contract or under any other contract presently or hereafter existing between the employer and the contractor and for this purpose all these contracts shall be considered one indivisible whole",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related: ____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["LIABILITY INSURANCES","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 11.0","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related: ____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["EFFECTING INSURANCES","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 12.0","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related: ____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D157*C157","v":{"v":0,"d":"R0.00"}}]
["Clause 13","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["No Clause",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SECURITY","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 14.0","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sub- clause 14.1 amend to read: The employer shall have the right to choose the security to be provided in terms of 14.3 or 14.4 as stated in the schedule. The contractor shall provide the security required or chosen by the employer in the schedule substantially in the format prescribed in the tender documents that the contractor submitted a tender offer. The required security shall be provided in the time period prescribed by the employer in the conditional letter of acceptance of the contractor’s tender offer.",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Amend sub-clause 14.3.1 Replace “twelve point five percent (12.5%)” with “ten percent (10%)”.",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Amend sub-clause 14.4.1 Replace “seven point five percent (7.5%)” with “ten percent(10%)”.",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Add a new sub-clause 14.7(a): The construction guarantee provided by the contractor shall remain valid for the term of the agreement until the defect’s liability period. In case of extensions, the security must also be extended or replaced by another of the same value, with an effective term equal to the term of extension. If the contractor fails to keep valid security for the duration of the agreement, the principal agent shall deduct an amount of 10% from each interim payment certificate and withhold the amount until the contractor provides a valid construction guarantee. Once the contractor provides the valid construction guarantee, the principal agent will then release the amount held from each payment certificate in the next payment certificate.  Amend the first sentence of sub-clause 14.7 to read: Should the contractor fail to furnish the security in terms of 14.1 or if the contractor’s security expires during the contract period, the employer, in his sole discretion, may either:”  ",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Amend sub-clause 14.7.1: Replace “two point five percent (2.5%)” with “five percent (5%)”.",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Add sub-clause 14.9 A payment reduction of ten (10%) of the value of each payment certificate up to a maximum of ten (10%) of the contract sum will be applied until practical completion. At practical completion the amount withheld will be reduced to five (5%), which amount will reduce to nil (0%) when the final account is issued.  ",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related: ____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["EXECUTION","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PREPARATION FOR AND EXECUTION OF THE WORKS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 15.0","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 15.1 is amended by replacing “principal agent” with “employer” ",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 15.1.1 is amended by replacing it with:",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["No clause",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["ACCESS TO THE WORKS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 16.0","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["CONTRACT INSTRUCTIONS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 17.0","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SETTING OUT OF THE WORKS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 18.0","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related: ____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["ASSIGNMENT","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 19.0","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 19.0 is amended by replacing it with the following:  19.1 The contractor does not cede, delegate or assign any of its rights or obligations to any person.  19.2 Notwithstanding the above, the employer may, on written notice to the contractor, cede and delegate, handover, its rights and obligations under this contract to a Related Party or a Client of the employer. On cession the Client becomes the employer and takes full responsibility. For the purpose hereof the above clause:",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["19.2.1 a “Related Party” means any entity that directly or indirectly, through one or more intermediaries, controls or is controlled by, or is under common control with the employer and includes any other “Organ of State” as defined in section 239 of the Constitution of the Republic of South Africa, 1996 and any entity or Organ of State for whom the Employer carries out the works or acts as an implementing agent, (“control” means the beneficial ownership of the majority in number of the issued equity of any entity (or the whole or majority of the entity’s assets), and/or the right or ability to direct or otherwise control the entity or the votes attaching to the majority of the entity’s equity and “controlled” or “under common control” shall have a similar meaning); and Client means the owner, funder and or sponsor of the project and or programme managed in terms of the MOA between the Client and DBSA",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D221*C221","v":{"v":0,"d":"R0.00"}}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOMINATED SUBCONTRACTORS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 20.0","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 20.1.3 is amended by replacing it with the following:",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["No clause",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SELECTED SUBCONTRACTORS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 21.0","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["EMPLOYER’S DIRECT CONTRACTORS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 22.0","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["CONTRACTOR’S DOMESTIC SUBCONTRACTORS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 23.0","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 23 is amended by the addition of the following:  Clause 23.3  The contractor may not subcontract the whole of the work without the written instruction or approval of the employer. In such event the employer may require the contractor to cede the contract to the subcontractor.”  Clause 23.4  The subcontractors appointed by the contractor to comply with the developmental and transformation requirements from the employer in terms of applicable legislation, including but not limited to the Preferential Procurement Policy Framework Act, 5 of 2000, and regulation thereto, will be domestic subcontractors for purposes of this agreement, and sub-clauses 23.1 and 23.2 will apply accordingly. ",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 23.5 The contractor shall submit the agreement for each subcontract to the Principal Agent and may redact all commercially sensitive information.  Clause 23.6  Contractors failure to pay Subcontractors  If the contractor fails to make payment of any amount due and payable to a subcontractor (“the Subcontractor debt”) and the Principal Agent considers that the subcontractor debt has an adverse impact(s) on the progress of the works or the obligations of the contractor under the agreement, the Principal Agent may request evidence of payment to the subcontractor. In the absence of such evidence, the employer may (at its own discretion) pay the subcontractor debt directly to the subcontractor concerned. Such payment is, for all purposes under the agreement, regarded as a payment made on behalf of the contractor and at the request of and with the approval and consent of the contractor, as a payment towards the contract sum. As such, payment to the contractor shall be less the payment to the subcontractor. All adverse effects as a result of or arising from the subcontractor debt does not entitle the contractor to any cost or time.",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related: ____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["COMPLETION","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PRACTICAL COMPLETION","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 24.0","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related: ____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["WORKS COMPLETION","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 25.0","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["FINAL COMPLETION","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 26.0","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["LATENT DEFECTS LIABILITY PERIOD","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 27.0","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SECTIONAL COMPLETION","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 28.0","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D285*C285","v":{"v":0,"d":"R0.00"}}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["REVISION OF DATE FOR PRACTICAL COMPLETION","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 29.0","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PENALTY FOR NON-COMPLETION","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 30.0","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 30 is amended by replacing reference to “36.3” at end of sentence with “36.0”",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PAYMENT","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["INTERIM PAYMENT TO THE CONTRACTOR","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 31.0","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 31.9 is amended by replacing the words \"seven (7) calendar days\" in the first line by the words \"thirty (30) calendar days”",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 31.12 is amended by deleting the following:",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Payment shall be subject to the employer giving the contractor a tax invoice for the amount due",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["ADJUSTMENT TO THE CONTRACT VALUE","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 32.0","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clauses 32.13 is amended with the addition of the following:  CPAP shall only be applicable to works that progress to later than twelve (12) months from commencement date. Where the period is prolonged beyond the first twelve months due to the delay or non- performance by the employer, the CPAP shall be applicable; however where the period is extended due contractor’s failure to perform or delay caused by the contractor CPAP shall not be applicable. The contract value is to be adjusted using CPAP indices. The base month to be used to calculate CPAP is tender closing date. The value of the certificates issued shall be adjusted in accordance with the JBCC Contract Price Adjustment Schedules, from the thirteenth month of the works.",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["RECOVERY OF EXPENSE AND LOSS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 33.0","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["FINAL ACCOUNT AND FINAL PAYMENT","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 34.0","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 34.13 is amended by deleting the words “subject to the employer giving the contractor a tax invoice for the amount due",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PAYMENT TO OTHER PARTIES","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 35.0","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["CANCELLATION","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["CANCELLATION BY EMPLOYER – CONTRACTOR’S DEFAULT","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 36.0","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D349*C349","v":{"v":0,"d":"R0.00"}}]
["Clause 36.1 is amended by the addition of the following clauses:",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["36.1.3 refuses or neglects to comply strictly with any of the conditions of contract",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["36.1.4 estate being sequestrated, liquidated or surrendered in terms of the insolvency laws in force within the Republic of South Africa",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["36.1.5 in the judgement of the employer, has engaged in corrupt or fraudulent practices in competing for or in executing the contract",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 36.3 is amended by replacing the words “principal agent” with “employer”",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 36.0 is amended by the addition of the following clause:",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["36.7 Notwithstanding any clause to the contrary, on cancellation of this agreement either by the employer or the contractor; or for any reason whatsoever, the contractor shall on written instruction, discontinue with the works on a date stated and withdraw himself from the site. The contractor shall not be entitled to refuse to withdraw from the works on the grounds of any lien or right of retention or on the grounds of any other right whatsoever",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["CANCELLATION BY EMPLOYER – LOSS AND DAMAGE","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 37.0","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 37.3.5 is amended by replacing “ninety (90)” with “one-hundred and twenty (120)”",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 37.0 is amended by the addition of the following clause:",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["37.5 Notwithstanding any clause to the contrary, on cancellation of this agreement either by the employer or the contractor; or for any reason whatsoever, the contractor shall on written instruction, discontinue with the works on a date stated and withdraw himself from the site. The contractor shall not be entitled to refuse to withdraw from the works on the grounds of any lien or right of retention or on the grounds of any other right whatsoever",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["CANCELLATION BY CONTRACTOR – EMPLOYER’S DEFAULT","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 38.0","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 38.5.4 is amended by replacing “ninety (90)” with “one-hundred and twenty (120)”",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 38.0 is amended by the addition of the following clause:",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["38.7 Notwithstanding any clause to the contrary, on cancellation of this agreement either by the employer or the contractor; or for any reason whatsoever, the contractor shall on written instruction, discontinue with the works on a date stated and withdraw himself from the site. The contractor shall not be entitled to refuse to withdraw from the works on the grounds of any lien or right of retention or on the grounds of any other right whatsoever",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["CANCELLATION – CESSATION OF THE WORKS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 39.0","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 39.3.5 is amended by the addition of the following at the end of the sentence: “within one hundred and twenty (120) working days of completion of such a report”",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["DISPUTE","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["DISPUTE SETTLEMENT","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 40.0","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 40.0 is amended by removing all state clause amendments  ",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SUBSTITUTE PROVISIONS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["STATE CLAUSES","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 41.0  Clause 41.1.3 Is amended to read \"CONSTRUCTION PERIOD\" means the period commencing on the date on which possession of site is given to the contractor as stated in the schedule and ending on the date of practical completion ","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D413*C413","v":{"v":0,"d":"R0.00"}}]
["Add  sub- clause 41.1.4 Notwithstanding any clause to the contrary, on cancellation of this agreement either by the employer or the contractor, or for any reason whatsoever, the contractor shall  on written instruction, discontinue with the works on a stated date and withdraw himself from the site. The contractor shall not be entitled to refuse to withdraw from the works on the grounds of any lien or right of retention or on the grounds of any other right whatsoever.",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clauses 21.0 Delete no clause  ",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 39.2 Is amended by replacing the third sentence with the following: The employer shall pay the contractor all amounts due in terms of the contract for work completed at the date of termination or cancellation in terms of this clause 39.2, including retention money after deducting any amounts due to the employer. The employer will also return any guarantees still valid to the contractor after such cancellation.",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clauses 39.2.1 to 39.2.3 Amend to no clause  ",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["CONTRACT VARIABLES","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["THE SCHEDULE (C1.2.2: CONTRACT SPECIFIC DATA)","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PRE-TENDER INFORMATION","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 42.0 Tenderers are referred to the document C1.2.2: Contract Specific Data for variables pertaining to this contract","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SECTION B: JBCC PRELIMINARIES","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["DEFINITIONS AND INTERPRETATION","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 1.1 Definitions and interpretation","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["DOCUMENTS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 2.1 Checking of documents","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 2.2 Provisional bills of quantities","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 2.3 Availability of construction documentation","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 2.4 Interests of agents","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 2.5 Priced documents","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:_________ __ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 2.6 Tender submission","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clause 2.6 is amended by replacing “JBCC Form of Tender” with “Form of Offer and Acceptance (C1.1)”",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["THE SITE","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 3.1 Defined works area","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 3.2 Geotechnical investigation","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D477*C477","v":{"v":0,"d":"R0.00"}}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 3.3 Site inspection","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Tenderers shall complete the Site Inspection Certificate included in the tender documents and return the same with the tender submission.",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 3.4 Existing premises occupied","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 3.5 Previous work – dimensional accuracy","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 3.6 Previous work – defects","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 3.7 Services – known","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 3.8 Services – unknown","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 3.9 Protection of trees","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 3.10 Articles of value","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 3.11 Inspection of adjoining properties","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["MANAGEMENT OF CONTRACT","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 4.1 Management of the works","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:_____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 4.2 Programme for the works","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related: ____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 4.3 Progress meetings","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related: ____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 4.4 Technical meetings","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related: ____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 4.5 Labour and plant records","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related: ____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SAMPLES, SHOP DRAWINGS AND MANUFACTURERS’ INSTRUCTIONS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D541*C541","v":{"v":0,"d":"R0.00"}}]
["B 5.1 Samples of materials","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 5.2 Workmanship samples","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 5.3 Shop drawings","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 5.4 Compliance with manufacturers’ instructions","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TEMPORARY WORKS AND PLANT","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 6.1 Deposits and fees","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 6.2 Enclosure of the works","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 6.3 Advertising","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 6.4 Plant, equipment, sheds and offices","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related: ____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 6.5 Main notice board","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related: ____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 6.6 Subcontractors’ notice board","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TEMPORARY SERVICES","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 7.1 Location","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 7.2 Water","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related: ____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 7.3 Electricity","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related: ____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 7.4 Telecommunication facilities","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related: ____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 7.5 Ablution facilities","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related: ____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D605*C605","v":{"v":0,"d":"R0.00"}}]
["PRIME COST AMOUNTS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 8.1 Responsibility for prime cost amounts","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["ATTENDANCE ON N/S SUBCONTRACTORS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 9.1 General attendance","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 9.2 Special attendance","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 9.3 Commissioning – fuel, water and electricity","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["FINANCIAL ASPECTS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 10.1 Statutory taxes, duties and levies","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 10.2 Payment for preliminaries  Option A will apply and the contractor will not have the right to select Option B","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 10.3 Adjustment of preliminaries  Option A will apply and the contractor will not have the right to select Option B","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clauses B10.3.1 and B10.3.2 are amended by replacing “within fifteen (15) working days of taking possession of the site” with “in his priced bills of quantities submitted with his tender offer”",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 10.4 Payment certificate cash flow","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["GENERAL","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 11.1 Protection of the works","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 11.2 Protection / isolation of existing / sectionally occupied works","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:_____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 11.3 Security of the works","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related: ___________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 11.4 Notice before covering work","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 11.5 Disturbance","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 11.6 Environmental disturbance","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D669*C669","v":{"v":0,"d":"R0.00"}}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 11.7 Works cleaning and clearing","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related: ___________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 11.8 Vermin","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 11.9 Overhand work","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 11.10 Instruction manuals and guarantees","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 11.11 As built information","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 11.12 Tenant installations","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SCHEDULE OF VARIABLES","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 12.1 Schedule of variables ","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["This schedule contains all variables referred to in this document and is divided into pre-tender and post-tender categories. The pre-tender category must be completed in full and included in the tender documents. Both the pre-tender and post-tender categories form part of these Preliminaries.",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Spaces requiring information must be filled in, shown as “not applicable” or deleted and not left blank. Where choices are offered, the non-applicable items are to be deleted. Where insufficient space is provided the information should be annexed hereto and cross-referenced to the applicable clause of the schedule. Key cross reference clauses are italicised in [ ] brackets",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PRE-TENDER INFORMATION","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 12.1.1 Provisional bills of quantities",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["[B2.2]The quantities are provisional",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 12.1.2 Availability of construction documentation",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["[B2.3]Construction documentation is complete",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 12.1.3 Interests of agents",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["[B 2.4] Details: NONE",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 12.1.4 Defined works area",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["[B 3.1] Details: Refer to C4 Site Information",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 12.1.5 Geotechnical investigation",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["[B 3.2] Details: Attached to this document  ",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 12.1.6 Existing premises occupied",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["[B 3.4] Specific requirements: N/A",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 12.1.7 Previous work – dimensional accuracy",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D733*C733","v":{"v":0,"d":"R0.00"}}]
["[B 3.5] Details: N/A",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 12.1.8 Previous work - defects",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["[B 3.6] Details: N/A",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 12.1.9 Services - known",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["[B 3.7] Details: N/A",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 12.1.10 Protection of trees",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["[B 3.9] Specific requirements: See Environment Management Pan ",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 12.1.11 Inspection of adjoining properties",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["[B 3.111] Specific requirements: NONE",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 12.1.12 Enclosure of the works",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["[B 6.2] Specific requirements:  The site must be suitably hoarded with at least a 1.8m high diamond mesh fence at all times with a limited number of restricted access points.",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 12.1.13 Offices",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["[B 6.4.3] Specific requirements:",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The contractor shall provide, keep clean and maintain and remove on completion of the works, air conditioned offices for the exclusive use of the Employer's agents comprising the following accommodation requirements:",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["6 x Site office which shall be used solely by the Employer’s Representative. Such an office shall comprise a minimum of 20m2 in area and 3m high, be ventilated, have good lamination, must be reasonably sound proof, and have a hard floor construction. It shall be furnished with a desk with lockable drawers on which drawings can be rolled open and on which there is sufficient writing space and a minimum of three temporary chairs. ",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Site boardroom which shall be used for site meetings and for the contractor’s use. Such an office shall comprise a minimum of 40m2 in area and 3m high, be ventilated, have good lamination, must be reasonably sound proof, and have a hard floor construction. It shall be furnished with a desk on which drawings can be rolled open and on which there is sufficient writing space and sufficient temporary chairs or benches to accommodate all persons present at site meetings. (Minimum 25 seater)  All windows are to be fitted with burglar bars and offices suitably insulated and ventilated and having good lighting.  The Contractor is required to provide latrine and ablution facilities for the exclusive use of the professional team and client.",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The following facilities will be supplied to the employers representatives: - 25 Hardhats for employers representatives visiting the site - 25 Safety (High visibility) jackets for employer representatives visiting the site - 25 sets of safety Goggles - 25 sets of earplugs (when applicable) - COVID-19 PPE requirements",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 12.1.14 Main notice board",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["[B 6.5] Specific requirements:",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The contractor shall provide, erect where directed, maintain and remove on completion of the works a notice board size 3 x 3m, constructed of suitable boarding with flat smooth surface and with edging bead 19mm thick round outer edges and projecting 12mm from face of boarding and rounded on front edge. The board shall be securely fixed to hoarding, where hoarding is provided, or fixed to and including a suitable supporting structure of timber or tubular posts and braces. ",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 12.1.15 Subcontractors’ notice board",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["[B6.6]A noticeboard is required: ",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 12.1.16 Water",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["[B7.2.1]Option A (by contractor)          ",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["[B7.2.2]Option B (by employer  - free of charge)            (yes/no)                No",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["[B7.2.3]Option C (by employer - metered)                      (yes/no)                No",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 12.1.17 Electricity",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["[B7.3.1]Option A (by contractor)                                    (yes/no)                Yes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["[B7.3.2]Option B (by employer  - free of charge)            (yes/no)                No",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["[B7.3.3]Option C (by employer - metered)",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 12.1.18 Telecommunications",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["[B7.4]Telephone","                                                  (yes/no)               Yes ",null,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D797*C797","v":{"v":0,"d":"R0.00"}}]
["[B7.4]Facsimile.                                                              (yes/no)                 Yes",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["[B7.4]E-mail                                                                    (yes/no)                Yes                                        ",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 12.1.19 Ablution facilities",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["[B7.5.1]Option A (by contractor)                                    (yes/no)              Yes",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["[B5.7.2]Option B (by employer)                                     (yes/no)               No",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 12.1.20 Protection of existing/sectionally occupied works",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["[B11.2]Protection is required                                          (yes/no)                No",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 12.1.21 Special attendance",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["[B 9.2] Subcontractor (1) details: NONE",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["[B 9.2] Subcontractor (2) details: NONE",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["[B 9.2] Subcontractor (3) details: NONE",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["[B 9.2] Subcontractor (4) details: NONE",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 12.1.22 Protection of the works",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["[B 11.1] Specific requirements: NONE",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 12.1.23 Disturbance",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["[B 11.5] Specific requirements:",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The contractor shall keep the site, structures, etc well watered during operations to prevent dust and shall provide and erect and remove on completion of the works all necessary temporary dust screens all to the satisfaction of the principal agent",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 12.1.24 Environmental disturbance",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["[B 11.6] Specific requirements: As per attached Environmental Management Plan",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["POST-TENDER INFORMATION","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 12.2 Payment of preliminaries",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["[B10.2.1]Option A (prorated)                                          (yes/no)              Yes",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["[B10.2.2]Option B (calculated)                                        (yes/no)              No",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 12.2.2 Adjustment of preliminaries",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["[B10.3.1]Option A (three categories)                               (yes/no)              Yes",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["[B10.3.2]Option B (detailed breakdown)                          (yes/no)               No",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["B 12.2.3 Additional agreed preliminaries items",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Details:",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SECTION C: SPECIFIC PRELIMINARIES","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Section C contains specific preliminary items which apply to this contract ",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["C1 CONTRACT DRAWINGS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The drawings issued with the tender documents do not comprise the complete set but serve as a guide only for tendering purposes and for indicating the scope of the work to enable the tenderer to acquaint himself with the nature and extent of the works and the manner in which they are to be executed","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D861*C861","v":{"v":0,"d":"R0.00"}}]
["Fixed: ____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["C2 TRADE NAMES","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Wherever a trade name for any product has been described in the bills of quantities, the tenderers attention is drawn to the fact that any other product of equal quality may be used subject to the written approval of the principal agent and specialist professional service provider where applicable. ","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed: ____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["C3 IMPORTED MATERIALS AND EQUIPMENT","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Where imported items are listed in the tender documents, the tenderer shall provide all the information called for, failing which the price of any such item, materials or equipment shall be excluded from currency fluctuations. (refer to Schedule of Imported Materials and Equipment to be completed by tenderer)","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Notwithstanding any provisions elsewhere regarding the adjustment of contract prices, the price of any item, material or equipment listed in terms of this clause shall be excluded from the Contract Price Adjustment Provisions (if applicable)",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed: ____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["HIV/AIDS AWARENESS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["It is required of the contractor to thoroughly study the HIV/AIDS Specification (PW 1544) of the Department that must be read together with and is deemed to be incorporated under this Section of the bills of quantities / lump sum document.  Provision for pricing of HIV/AIDS awareness is made under items C11.1 to C11.5 hereafter and it is explicitly pointed out that all requirements of the aforementioned specification are deemed to be priced hereunder, as the said items represent the only method of measurement and no additional items or extras to the contract in this regard shall be entertained",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The contractor must take note that compliance with the HIV/AIDS Specification is compulsory.  In the event of partial or total non-compliance, the principal agent, notwithstanding the provisions of Clause 31 of “Section 1: Preliminaries” or any other clause to the contrary, reserves the right to delay issuing any progress payment certificate until the contractor provides satisfactory proof of compliance.  The contractor shall not be entitled to any compensation of whatsoever nature, including interest, due to such delay of payment",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["C4.1 AWARENESS CAMPAIGN ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Selection, appointment, briefing and making available of an Awareness Campaign including provision of all relevant services, all in accordance with the HIV/AIDS Specification","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:_____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["C4.2 AWARENESS WORKSHOPS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Selection and appointment of a competent Service Provider approved by the principal agent, provision of a Service Provider Workshop Plan and a suitable venue, conducting of awareness workshops by means of traditional and/or modern multi-media techniques, including follow-up courses, making available all tuition material and performing assessment procedures, all in accordance with the HIV/AIDS Specification","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:_____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["C4.3 POSTERS, BOOKLETS, VIDEOS, ETC.","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Provision, displaying, maintaining and replacing when necessary of four plastic laminated posters, booklets and educational videos, etc. for the duration of the construction period, all in accordance with the HIV/AIDS Specification","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:_____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["C4.4 ACCESS TO CONDOMS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Provision and maintenance of condom dispensers fixed in position, including male and female condoms, replenishing male and female condoms on a daily basis as required for the duration of the construction period, all in accordance with the HIV/AIDS Specification","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:_____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["C4.5 MONITORING","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Monitoring HIV/AIDS awareness of workers, providing the principal agent with access to information including making available all reports, thoroughly completed and reflecting the correct information, for the duration of the construction period and close out, all in accordance with the HIV/AIDS Specification","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related: ____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["C5 OCCUPATIONAL HEALTH AND SAFETY ACT","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The contractor shall comply with all the requirements set out in the Construction Regulations, 2014 issued under the Occupational Health and Safety Act, 1993 (Act No.85 of 1993).","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["It is required of the contractor to thoroughly study the Health and Safety Specification that must be read together with and is deemed to be incorporated under this Section of the bills of quantities / lump sum document.",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The contractor must take note that compliance with the Occupational Health and Safety Act, Construction Regulations and Health and Safety Specification is compulsory.  In the event of partial or total non-compliance, the principal agent, notwithstanding the provisions of Clause 31 of “Section 1: Preliminaries” or any other clause to the contrary, reserves the right to delay issuing any progress payment certificate until the contractor provides satisfactory proof of compliance.  The contractor shall not be entitled to any compensation of whatsoever nature, including interest, due to such delay of payment.",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Provision for pricing of the Occupational Health and Safety Act, Construction Regulations and Health and Safety Specification is made under this clause and it is explicitly pointed out that all requirements of the aforementioned are deemed to be priced hereunder and no additional claims in this regard shall be entertained.",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related: ____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D925*C925","v":{"v":0,"d":"R0.00"}}]
["C6 COVID-19 MONITORING & AWARENESS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The contractor shall comply with all the requirements set by Government and as required depending on the National Alert Level implemented at the time of construction.  COVID-19 awareness and safe operating procedures must include, but are not limited to, daily screening of all workers and site visitors on arrival and departure, record keeping, daily awareness reminders, awareness posters, sanitising stations, PPE, etc.  The contractor shall price opposite this item for the development and implementation of a COVID-19 plan and appointment of COVID-19 officer. ","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related: ____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["C7 SUBCONTRACTING AS A CONDITION OF TENDER","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The successful bidder shall be required to subcontract a minimum of 30% of the value of the Contract including labour and materials to EME’S or/and QSE’S enterprises determined in terms of section 9(1) of the Broad-Based Black Economic Empowerment Act.  These sub-contractors can be selected from the CIDB database who are registered on the CSD for the purposes of compliance. Bidders shall make allowance in their preliminaries for any additional costs in this regard, for example, for the preparation of work packages, management of the subcontractors including site supervision, drafting and conclusion of subcontract agreements, subcontractor OHS plan approvals, etc., that may arise due to this commitment. ","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["C8 GENERAL LABOUR MINIMUM TARGETS  ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["General Labour minimum targetsIt is mandatory that tenderers/bidders employ the minimum stipulated personnel on the contracts for the local community where the project is being implemented. This employment is outside the existing employees of the tenderers/bidders. For the general labour force, the minimum number of people to be employed for the duration of the Project will be calculated from the formula below.            ","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Tenderers are to also note that it is an explicit condition of this tender that all unskilled labourers on the project are to be employed from the local community.  The Contractor is therefore expected in general to maximise the involvement of the local community. Take note that the local labour employed must not be paid lower than the minimum approved Municipal rates in that district or area.  The Contractor shall be required to submit employment data on a monthly basis to the Project Manager.  Should the contractor at Works Completion, be in default by non-attainment of the above mentioned labour intensive targets, the Employer shall have the right to, without prejudice of any other rights, apply a penalty of not exceeding 5% of the contract sum.",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["C9 LOCAL LABOUR ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["It is the intention that this Contract should make maximum use of the local labour force that is presently under-employed.  To this end the Contractor shall limit the utilisation on the Contract of non-local employees to that of key personnel only and to employ and train local labour to the extent necessary for the execution and completion of this Contract.  The Contractor shall fill in the form entitled Key Personnel in the Forms to be completed by the Bidder.  The data stated on the above-mentioned form will be strictly monitored during the Contract period and any deviations there from shall be subject to the prior approval of the Principal Agent, which approval shall not be unreasonably withheld.  The employment of casual labour will be done in co-operation with community leaders and local structures.  The bidder shall ensure that all remuneration paid to employees is in line with the relevant sectorial determination in terms of the Basic Conditions of Employment Act, No 75 of 1997, as determined by the Department of Labour.","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["C10 LOCAL MATERIAL ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Regarding procurement of materials, local is hereby defined as the district in which the project(s)  is/are located. The minimum target for materials sourced locally is 20% of the contract value","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["C11 NON ACCREDITED TRAINING OF LABOUR ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The Contractor shall provide all the necessary on-the-job training to targeted labour to enable such labour to master the basic work techniques required to undertake the work in accordance with the requirements of the contract in a manner that does not compromise worker health and safety.  The contractor shall be responsible for scheduling the training of workers and shall take all reasonable steps to ensure that each beneficiary is provided with a minimum of six (6) days of formal training if he/she is employed for 3 months or less and a minimum of ten (10) days if he/she is employed for 4 months or more.  The Contractor shall do nothing to dissuade targeted labour from participating in training programmes.  Proof of compliance with all the requirements must be provided by the Contractor to the Employer prior to submission of the final payment certificate.","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["C12 ENVIRONMENTAL MANAGEMENT PLAN ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The contractor shall comply with all the requirements in the environmental management plan attached to this document. It is required of the contractor to thoroughly study attached environmental management plan. The contractor must take note that compliance with the environmental management plan is compulsory. In the event of partial or total non-compliance, the principal agent, notwithstanding the provisions of Clause 31 of “Section 1: Preliminaries” or any other clause to the contrary, reserves the right to delay issuing any progress payment certificate until the contractor provides satisfactory proof of compliance.  The contractor shall not be entitled to any compensation of whatsoever nature, including interest, due to such delay of payment. Provision for pricing of all the main contractors cost in this regard is made under this clause and are deemed to be priced hereunder and no additional claims in this regard shall be entertained. ","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixed:____________ Value related:____________ Time related:____________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TOTAL SECTION 1 CARRIED TO FINAL SUMMARY",{"$nulls":3},{"$f":"SUM(E2:E969)","v":{"v":0,"d":"0.00"}}]
[null,null,0,null,{"v":0,"d":"R0.00"}]
["SECTION 2","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NEW HOSPITAL ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["BILL NO 1","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["FOUNDATIONS (PROVISIONAL)","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PREAMBLES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Preambles for Trades as defined in Scope of Work (C3.1 Item 4.1 & Item 4.2)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TRADE NAMES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Any reference to trade names in the Bills of Quantities or  Architect's specification or drawings shall deem to mean \"or similar and approved\"",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SUPPLEMENTARY PREAMBLES","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D989*C989","v":{"v":0,"d":"R0.00"}}]
["Nature of material to be excavated","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["A geotechnical report has been carried out on site by the engineer and the report is available at the offices of the Engineers. Descriptions of excavations shall be deemed to include all ground conditions classifiable as \"earth\" described in the above report and where conditions of a more difficult character are indicated these are separately measured",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Carting away of excavated material","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Descriptions of carting away of excavated material shall be deemed to include loading excavated material onto trucks directly from the excavations or, alternatively, from stock piles situated on the building site",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavation for working space in rock","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Notwithstanding the Standard System of Measuring Building Work, excavation for working space in rock will be measured in cubic metres to the extent executed and given as \"extra over\" bulk excavation or trench and hole excavation as the case may be",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Filling","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Notwithstanding the reference to prescribed multiple handling in clause 1 page 6 of the Standard System of Measuring Building Work, prices for filling and backfilling shall include for all selection and any necessary multiple handling of material",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Testing","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Prices for filling are to include for all necessary density tests in accordance with SABS 1200D",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Subterranean water","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["No information regarding subterranean water is available. The tenderer must acquaint himself of the presence and depth of subterranean water and allow therefore in his prices ____________________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 104 for JBCC CPAP purposes ",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["EARTHWORKS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["EXCAVATION, FILLING, ETC","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavation in earth or compacted filling not exceeding 2m deep","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Trenches","m3",7917,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Holes","m3",5642,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavation in earth or compacted filling  exceeding 2m not exceeding 4m deep","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Trenches","m3",249,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Holes","m3",4846,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavation in earth or compacted filling  exceeding 4m not exceeding 6m deep","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Trenches","m3",190,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Holes","m3",57,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over excavations in earth for excavation in","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Soft rock","m3",2270,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Hard rock","m3",1195,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over all excavations for carting away","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Surplus material from excavations and/or stock piles on site to a dumping site to be located by the contractor","m3",8774,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Risk of collapse of excavations","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sides of trench and hole excavations not exceeding 1,5m deep","m2",12964,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but exceeding 1,5m deep ","m2",20328,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D1053*C1053","v":{"v":0,"d":"R0.00"}}]
["Keeping excavations free of water","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Keeping excavations free of water ","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Selected earth filling obtained from the excavations and/or prescribed stock piles on site in layers of 150mm thick compacted to 93% Mod AASHTO density","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Backfilling to trenches, holes, etc","m3",12463,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Selected earth filling obtained from the excavations and/or prescribed stock piles on site in layers of 150mm thick compacted to 95% Mod AASHTO density","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Under floors, steps, pavings, etc","m3",6621,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Approved G5 filling supplied and carted on by the Contractor, compacted in layers not exceeding 150mm to 95% Mod. AASHTO density","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Under solid floors ","m3",6621,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["20mm Thick coarse river sand filling supplied by the contractor","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Under floors etc","m2",44142,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Compaction of surfaces ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Compaction of ground surface under surface beds etc including scarifying for a depth of 150mm, breaking down oversize material, adding suitable material where necessary and compacting to 93% Mod AASHTO density","m2",44142,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SOIL INSECTICIDE","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Soil insecticide in accordance with SANS 5859","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Under floors etc including forming and poisoning shallow furrows against foundation walls etc, filling in furrows and ramming (Certificate to be supplied before payment is made)","m2",44142,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["To bottoms and sides of trenches and holes (Certificate to be supplied before payment is made)","m2",23765,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 110 for JBCC CPAP purposes ",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["UNREINFORCED CONCRETE CAST AGAINST EXCAVATED SURFACES ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["15MPa/19mm concrete","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blinding under footings and bases","m3",579,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["REINFORCED CONCRETE CAST AGAINST EXCAVATED SURFACES ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["30MPa/19mm concrete","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Strip footings","m3",1558,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Bases ","m3",3178,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Walls","m3",824,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Floor channels","m3",159,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["50MPa/19mm concrete","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Columns in foundations","m3",829,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TEST BLOCKS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Making and testing set of three 150 x 150 x 150 mm strength test cubes","Sets",130,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 111 for JBCC CPAP purposes ",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["ROUGH FORMWORK (DEGREE OF ACCURACY II)","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D1117*C1117","v":{"v":0,"d":"R0.00"}}]
["Rough formwork to sides","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Square Columns","m2",16,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Rectangular columns ","m2",6475,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Walls in floor channels","m2",941,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Walls not exceeding 3.5m high","m2",6227,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Walls exceeding 3.5m and not exceeding 5m high","m2",699,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Rough formwork to circular columns ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["380mm Diameter circular column 1.75m High","No",26,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["400mm Diameter circular column 1.45m high","No",36,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Movement  joints etc.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["10mm Jointex  in vertical joint between concrete and brickwork not exceeding 300mm wide or high ","m",1546,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 114 for JBCC CPAP purposes ",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["REINFORCEMENT","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Mild tensile steel rod reinforcement to structural concrete ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["8mm Diameter bars","t",95.61,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["High tensile steel rod reinforcement to structural concrete ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["10mm Diameter bars","t",204.81,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["12mm Diameter bars","t",242.88,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["16mm Diameter bars","t",185.92,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["20mm Diameter bars","t",101.57,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 116 for JBCC CPAP purposes ",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["MASONRY","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Brickwork (14Mpa nominal compressive strength) in 2:1 cement mortar","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["One brick walls","m2",86,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but circular on plan ","m2",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["330mm Cavity walls formed of two half brick skins and 110mm cavity filled with 15 MPa concrete, including wire ties","m2",6418,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but circular on plan","m2",40,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Brickwork reinforcement","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["75mm Wide reinforcement built in horizontally","m",38990,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150mm Wide reinforcement built in horizontally","m",254,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but circular on plan ","m",13,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Galvanized hoop iron cramps, ties etc.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D1181*C1181","v":{"v":0,"d":"R0.00"}}]
["1.6 x 32 x 400mm long Galvanised hoop irons ties fixed to concrete and built into brickwork  ","No",4546,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["FACE BRICKWORK","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Corobrik Imperial FBX face brick, size 222 x 106 x 73mm, manufactured in accordance with 227:2007 (PC Amount of R7,500.00 per thousand bricks delivered to site, excluding VAT) pointed with flush horizontal and vertical joints ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over brickwork for face brickwork ","m2",10,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 120 for JBCC CPAP purposes ",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["WATERPROOFING ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sikaguard 905 waterproofing in accordance with the manufacturer`s specifications. (Sika 051 430 0333) as per detail drawing HDG - TYP-042-036 or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Waterproofing spayed to foundation walls ","m2",12478,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 142 for JBCC CPAP purposes ",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["EXTERNAL PLASTER","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["One coat 1:6 cement plaster on brickwork","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On walls","m2",3192,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On circular walls","m2",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 152 for JBCC CPAP purposes ",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PAINTWORK","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Prepare surfaces and remove all loose material and rinse.  Surfaces to be dry, sound and clean and cured for stipulated 28 or 14 days as stated with a moisture content, measured with a Doser Hygrometer of BD 2 scale - 8%.  Apply with one coat unreduced 100% pure acrylic emulsion water based Versus primer with two coats 100% pure acrylic water based Versus Surewall paint enhanced with marble aggregate, fillers and fungicides or similar approved. All to manufacturer’s detailed specifications. TVOC limits (g/L of product) to be compliant to TVOC limits in Table IEQ13.1 for Green Star PEB - Custom Healthcare. Colour to Architect’s selection","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["External plastered walls ","m2",3195,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TOTAL FOUNDATIONS ",{"$nulls":3},{"$f":"SUM(E971:E1215)","v":{"v":0,"d":"0.00"}}]
[null,null,0,null,{"v":0,"d":"R0.00"}]
["SECTION 2","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NEW HOSPITAL ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["BILL NO 2","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["CONCRETE FORMWORK AND REINFORCEMENT","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PREAMBLES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Preambles for Trades as defined in Scope of Work (C3.1 Item 4.1 & Item 4.2)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TRADE NAMES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Any reference to trade names in the Bills of Quantities or  Architect's specification or drawings shall deem to mean \"or similar and approved\"",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SUPPLEMENTARY PREAMBLES","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Type of cement","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["All cement used in concrete work is to be OPC cement, no cement containing fly ash will be allowed",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cost of tests","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The costs of making, storing and testing of concrete test cubes  shall include the cost of providing cube moulds necessary for the purpose, for testing costs and for submitting reports on the tests to the Representative/Agent. The testing shall be undertaken by an independent firm or institution nominated by the contractor to the approval of the Representative/Agent.  (Test cubes are measured separately)",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Breeze concrete","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D1245*C1245","v":{"v":0,"d":"R0.00"}}]
["Breeze concrete shall consist of twelve parts clean dry furnace ash, free from coal or other foreign matter, to one part cement (1:12); the ash graded up to particles which will pass a 16,5mm ring from a minimum which fails to pass a 4,75mm mesh.  The finer materials from the screening are to be first mixed with the cement into a mortar and the ash added afterwards and thoroughly incorporated",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Lightweight concrete","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Lightweight concrete shall have a density of 600kg/m3 for the top 50mm and 400kg/m3 for the remaining thickness.  The minimum thickness at outlets, channels, etc shall be 50mm",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Formwork","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Descriptions of formwork shall be deemed to include use and waste only (except where described as \"left in\" or \"permanent\"), for fitting together in the required forms, wedging, plumbing and fixing to true angles and surfaces as necessary to ensure easy release during stripping and for reconditioning as necessary before re-use",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The vertical strutting shall be carried down to such construction as is sufficiently strong to afford the required support without damage and shall remain in position until the newly constructed work is able to support itself",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Formwork to soffits of solid slabs etc shall be deemed to be to slabs not exceeding 250mm thick unless otherwise described",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Formwork to soffits of slabs, beams, etc shall be deemed to be propped up exceeding 1,5m and not exceeding 3,5m high unless otherwise described",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Formwork to sides of bases, pile caps, ground beams, etc will only be measured where it is prescribed by the engineer for design reasons.  Formwork necessitated by irregularity or collapse of excavated faces will not be measured and the cost thereof shall be deemed to be included in the allowance for taking the risk of collapse of the sides of the excavations, provision for which is made in \"Earthworks\"",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Smooth formwork","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["All smooth formwork must be cleaned, all unevenness removed, properly prepared and then finished with a final coat of cementitious paint to give a smooth and even finish",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 110 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["CONCRETE","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["REINFORCED CONCRETE ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["25 MPa/19 mm concrete in","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Surface beds on waterproofing","m3",2769,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ramps on waterproofing","m3",43,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Walls","m3",2981,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Retaining walls","m3",399,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["30 MPa/19 mm concrete in","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ground slabs on waterproofing","m3",7255,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Slabs","m3",23182,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Stepped slabs including beams and inverted beams","m3",60,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ramps","m3",364,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Stairs including landings","m3",375,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Beams and inverted beams","m3",2673,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["50 MPa/19 mm concrete in","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Columns","m3",2362,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TEST BLOCKS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Making and testing set of three 150 x 150 x 150 mm strength test cubes","No",857,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["CONCRETE SUNDRIES","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Finishing top surface of concrete smooth with a wood float ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D1309*C1309","v":{"v":0,"d":"R0.00"}}]
["Surface beds, slabs, etc to falls and currents","m2",6093,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 111 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sleeves","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Vertical sleeves through concrete slabs ","H4",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["200mm Diameter uPVC sleeves not exceeding 340mm long","No",59,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["250mm Diameter uPVC sleeves not exceeding 340mm long","No",59,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["300mm Diameter uPVC sleeves not exceeding 340mm long","No",59,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["FORMWORK","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["ROUGH FORMWORK (DEGREE OF ACCURACY II)","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Rough formwork to sides","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Retaining walls exceeding 3.5m and not exceeding 5m high","m2",2662,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Walls not exceeding 3.5m high","m2",3688,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but circular on plan exceeding 1 meter radius","m2",142,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Walls exceeding 3.5m and not exceeding 5m high","m2",16625,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Walls exceeding 5m and not exceeding 6.5m high","m2",319,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Inner face of shaft walls (shaft approximately 3m x 3m internally and total wall height exceeding 14m and not exceeding 15.5m)","m2",197,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Inner face of shaft walls (shaft approximately 3m x 3m internally and total wall height exceeding 17m and not exceeding 18.5m)","m2",1761,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Outer face of walls flush with perimeter of concrete structure (total wall height exceeding 14m and not exceeding 15.5m)","m2",208,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Outer face of walls flush with perimeter of concrete structure (total wall height exceeding 17m and not exceeding 18.5m)","m2",1864,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Inverted beams not exceeding 3.5m high","m2",1787,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but circular on plan exceeding 1 meter radius","m2",22,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Inverted beams exceeding 3.5m and not exceeding 5m high","m2",1339,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but circular on plan exceeding 1 meter radius","m2",43,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Inverted beams exceeding 5m and not exceeding 6.5m high","m2",10,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Inverted beams exceeding 6.5m and not exceeding 8m high","m2",39,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but circular on plan exceeding 1 meter radius","m2",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Inverted beams set sloping not exceeding 3.5m high","m2",93,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Inverted beams set sloping exceeding 3.5m and not exceeding 5m high","m2",177,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Beams set sloping not exceeding 3.5m high","m2",120,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Beams set sloping exceeding 3.5m not exceeding 5m high","m2",262,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Beams not exceeding 3.5m high","m2",2552,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but circular on plan exceeding 1 meter radius","m2",32,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D1373*C1373","v":{"v":0,"d":"R0.00"}}]
["Beams exceeding 3.5m not exceeding 5m high","m2",2247,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but circular on plan exceeding 1 meter radius","m2",67,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Beams exceeding 5m not exceeding 6.5m high","m2",21,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but circular on plan exceeding 1 meter radius","m2",13,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Beams exceeding 6.5m not exceeding 8m high","m2",61,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Square columns not exceeding 3.5m high","m2",24,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Square columns exceeding 3.5m and not exceeding 5m high","m2",114,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Rectangular columns not exceeding 3.5m high","m2",4813,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Rectangular columns exceeding 3.5m and not exceeding 5m high","m2",17163,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Rectangular columns exceeding 5m and not exceeding 6.5m high","m2",302,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Rectangular columns exceeding 6.5m and not exceeding 8m high","m2",176,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Rectangular columns exceeding 11m and not exceeding 12.5m high","m2",386,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Rectangular columns exceeding 14m and not exceeding 15.5m high","m2",161,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Rectangular columns exceeding 15.5m and not exceeding 17m high","m2",246,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["L-shaped columns not exceeding 3.5m high","m2",50,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["L-shaped columns exceeding 3.5m and not exceeding 5m high","m2",149,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Irregular L-shaped columns not exceeding 3.5m high","m2",97,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Irregular L-shaped columns exceeding 3.5m and not exceeding 5m high","m2",310,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Irregular L-shaped columns exceeding 15.5m and not exceeding 17m high","m2",108,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Tapering side of column tapering from 650mm bottom  to 900mm top, exceeding 6.5m and not exceeding 8m high","m2",213,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Raking side of tapering columns exceeding 6.5m and not exceeding 8m high","m2",30,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Edges, risers, ends and reveals not exceeding 300mm high ","m",7467,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but circular on plan exceeding 1 meter radius","m",141,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sloping and stepped outer edges of stairs not exceeding 300mm high ","m",1568,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Rough formwork to soffits of:","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Slabs not exceeding 250mm thick, propping not exceeding 3,5m high","m2",205,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Slabs exceeding 250mm and not exceeding 500mm thick, propping not exceeding 3,5m high","m2",7087,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Slabs exceeding 250mm and not exceeding 500mm thick, propping exceeding 3,5m and not exceeding 5m high","m2",69382,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Slabs exceeding 250mm and not exceeding 500mm thick, propping exceeding 5m and not exceeding 6.5m high","m2",126,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Slabs exceeding 250mm and not exceeding 500mm thick, propping exceeding 6.5m and not exceeding 8m high","m2",264,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Slabs exceeding 250mm and not exceeding 500mm thick, propping exceeding 11m and not exceeding 12.5m high","m2",19,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Slabs exceeding 250mm and not exceeding 500mm thick, propping exceeding 15.5m and not exceeding 17m high","m2",82,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D1437*C1437","v":{"v":0,"d":"R0.00"}}]
["Slabs with sloping soffits exceeding 250mm and not exceeding 500mm, propping not exceeding 3,5m high","m2",1422,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Slabs with sloping soffits exceeding 250mm and not exceeding 500mm, propping exceeding 3,5m and not exceeding 5m high","m2",229,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Slabs over shafts exceeding 250mm and not exceeding 500mm thick, propping exceeding 14m and not exceeding 15.5m high","m2",20,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Slabs over shafts exceeding 250mm and not exceeding 500mm thick, propping exceeding 17m and not exceeding 18.5m high","m2",67,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cantilever slabs exceeding 250mm and not exceeding 500mm thick, propping exceeding 3.5m and not exceeding 5m high","m2",79,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cantilever slabs exceeding 250mm and not exceeding 500mm thick, propping exceeding 5m and not exceeding 6.5m high","m2",225,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cantilever slabs exceeding 250mm and not exceeding 500mm thick, propping exceeding 11m and not exceeding 12.5m high","m2",110,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Landings not exceeding 250mm thick, propping not exceeding 3,5m high","m2",1133,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Stairs with sloping soffits not exceeding 250mm thick, propping not exceeding 3,5m high","m2",658,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Rough formwork to sides and soffits","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Beams not exceeding 3.5m high","m2",26,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Isolated beams not exceeding 3.5m high ","m2",14231,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but circular on plan exceeding 1 meter radius","m2",18,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Isolated beams exceeding 3.5m and not exceeding 5m high ","m2",583,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Isolated beams exceeding 5m and not exceeding 6.5m high ","m2",245,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SMOOTH FORMWORK (DEGREE OF ACCURACY II) ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["All smooth formwork must be cleaned, all unevenness removed, properly prepared and then finished with a final coat of cementitious paint to give a smooth and even finish",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Formwork to sides","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Rectangular columns not exceeding 3.5m high","m2",38,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Rectangular columns exceeding 3.5m and not exceeding 5m high","m2",2212,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Formwork to circular columns ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["380mm Diameter circular column 3.40m high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["380mm Diameter circular column 3.78m high","No",17,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["380mm Diameter circular column 4.12m high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["400mm Diameter circular column 3.20m high","No",36,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Boxing in smooth formwork to form:","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["20 x 20mm Vertical chamfer at corners ","m",4965,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PERMANENT FORMWORK","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Gallery slab permanent formwork stepped to soffit and sides","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Stepped gallery slab","m2",226,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["MOVEMENT JOINTS, ETC","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Saw cut joints","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D1501*C1501","v":{"v":0,"d":"R0.00"}}]
["3 x 40mm Saw cut joints in top of concrete surface bed ","m",1936,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Expansion joints formed of jointex","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["10mm Jointex in vertical joint between concrete surfaces exceeding 300mm ","m2",353,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["10mm Jointex in vertical joint between concrete surfaces not exceeding 300mm high or wide","m",1500,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 114 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["REINFORCEMENT (PROVISIONAL)","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Mild steel rod reinforcement to structural concrete ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["8mm Diameter bars","t",305.07,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["High tensile steel rod reinforcement to structural concrete ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["10mm Diameter bars","t",1382.73,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["12mm Diameter bars","t",1765.92,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["16mm Diameter bars","t",1192.57,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["20mm Diameter bars","t",345.43,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fabric reinforcement","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Type 245 fabric reinforcement in concrete surface beds, slabs, etc.","m2",20807,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TOTAL CONCRETE FORMWORDAND REINFORCEMENT ",{"$nulls":3},{"$f":"SUM(E1217:E1531)","v":{"v":0,"d":"0.00"}}]
[null,null,0,null,{"v":0,"d":"R0.00"}]
["SECTION 2","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["BILL NO 3","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["MASONRY","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PREAMBLES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Preambles for Trades as defined in Scope of Work (C3.1 Item 4.1 & Item 4.2)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TRADE NAMES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Any reference to trade names in the Bills of Quantities or  Architect's specification or drawings shall deem to mean \"or similar and approved\"",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SUPPLEMENTARY PREAMBLES","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sizes in descriptions","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Where sizes in descriptions are given in brick units, \"one brick\" shall represent the length and \"half brick\" the width of a brick",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Wall ties","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Descriptions of solid walls (except if built in English bond) and cavity walls shall be deemed to include metal wall ties complying with SABS 28 and of the butterfly or of the modified PWD type, of the required length with each end built at least 75mm deep into brickwork, spaced at not more than 1m centres alternatively to every third course of brickwork",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cavity walls, etc.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Descriptions of cavity walls shall be deemed to include leaving every fifth perpend of the bottom course of the external skin open as a weep hole",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Face bricks","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Bricks shall be ordered timeously to obtain uniformity in size and colour",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D1565*C1565","v":{"v":0,"d":"R0.00"}}]
["Pointing","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Descriptions of recessed pointing to fair face brickwork and face brickwork shall be deemed to include square recessed, hollow recessed, weathered pointing, etc.",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 116 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SUPERSTRUCTURE","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Brickwork of clay bricks in 6:1 cement mortar","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Half brick walls","m2",12314,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Half brick walls built against brickwork","m2",490,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Half brick fire walls","m2",158,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Half brick linings tied to concrete","m2",161,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Half brick walls in beam filling ","m2",151,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["One brick walls","m2",68721,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["One brick walls built against brickwork","m2",586,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["One brick walls circular on plan","m2",357,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["One brick walls tied to concrete","m2",166,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["One brick fire walls","m2",16350,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["One brick walls in beam filling ","m2",1503,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["One and a half brick wall","m2",441,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["One brick x 440mm wide duct pier attached","m",2032,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["One brick x 440mm wide duct pier attached to concrete","m",1260,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["BRICKWORK SUNDRIES","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Splayed mortar fillet 115mm wide x 85mm high to form window sill ","m",5831,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Movement joints, etc.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["10mm Jointex  in vertical joint built in vertically between brick and concrete surfaces not exceeding 300mm wide, including polysulphide sealer etc.","m",26594,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Brick reinforcement ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["75mm Wide reinforcement built in horizontally ","m",40352,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150mm Wide reinforcement built in horizontally ","m",304550,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150mm Wide reinforcement built in horizontally circular on plan","m",1047,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Prestressed concrete lintels","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["105mm Wide lintel in lengths not exceeding 3m","m",6113,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["105mm Wide lintels in lengths exceeding 3m and not exceeding 4,5m","m",267,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["105mm Wide lintels in lengths exceeding 4,5m and not exceeding 6m","m",159,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["105mm Wide lintels in lengths exceeding 6m and not exceeding 7.5m","m",43,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D1629*C1629","v":{"v":0,"d":"R0.00"}}]
["105mm Wide lintels in lengths exceeding 7.5m and not exceeding 9m","m",18,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Precast concrete finished smooth on exposed surfaces including bedding, jointing and pointing","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["450 x 100mm Thick wire mesh reinforced precast seat slabs in 1000mm lengths, with 20mm rounded edge along one of the top edges, bedded on top of dwarf walls (dwarf walls elsewhere) with 10mm mortar flush joints between panels, including bedding edges at ends and along one side","m",15,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Turning pieces to lintels etc","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["220mm Wide turning pieces","m",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Galvanized hoop iron cramps, ties, etc.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["1.6 x 32 x 400mm long galvanised hoop irons ties fixed to concrete and built into brickwork ","No",146263,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["1900 x 550mm Opening through 220mm wall including necessary lintels ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sleeves","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Horizontal sleeves through brick/concrete walls","H4",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["200mm Diameter uPVC sleeves not exceeding 300mm long","No",59,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["250mm Diameter uPVC sleeves not exceeding 300mm long","No",59,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["300mm Diameter uPVC sleeves not exceeding 300mm long","No",59,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["FACE BRICKWORK","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Corobrik Imperial FBX face brick, size 222 x 106 x 73mm, manufactured in accordance with 227:2007 (PC Amount of R7,500.00 per thousand bricks delivered to site, excluding VAT) pointed with recessed horizontal and vertical joints ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Half brick face brickwork","m2",88,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over brickwork for face brickwork","m2",5653,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Corobrik Imperial FBX face brick, size 222 x 106 x 73mm, manufactured in accordance with 227:2007 (PC Amount of R7,500.00 per thousand bricks delivered to site, excluding VAT) pointed with flush horizontal and vertical joints ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Half brick face brickwork","m2",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over brickwork for face brickwork","m2",625,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Brick-on-edge header course copings, sills, etc. of face bricks pointed with recessed joints on all exposed faces","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["220mm Copings on top of one brick walls","m",15,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Brick on edge header course lintel 220mm wide pointed on face and 115mm soffit ","m",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Brick on edge header course internal window sill 110mm wide, including pointing on all exposed sides including cutting of brickwork underneath.","m",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["BLOCKWORK","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["DSM Masonry M150 series in class 6:1 cement mortar, pointed with flush recessed horizontal and vertical joints or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["140 x 390 x 190mm Breeze block","m2",93,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["GLASS BLOCK WALLS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["80 x 240 x 240mm \"Clearview 248\" glass blocks bedded and jointed in slow-setting class 2 mortar with continuous joints in both directions and pointed in tinted mortar on both sides with recessed horizontal and vertical joints and sealing with elastic sealant or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["240mm Walls circular on plan","m2",180,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sundries","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["240mm Wide horizontal slip joints below glass blocks consisting of two layers type FV dampproofing","m",45,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D1693*C1693","v":{"v":0,"d":"R0.00"}}]
["6 x 240mm Wide expanded polystyrene (density 33kg per m3) horizontally and vertically between glass blocks and structure","m",206,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["8mm Diameter galvanised mild steel bar reinforcement horizontally and vertically","t",0.285,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SAMPLE PANEL ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Construct a facebrick sample panel 2m long x 1,5m high of one brick wall in cement mortar faced and pointed on both sides in stretcher bond and with brick-on-edge coping to top and both sides including necessary excavations for and including 15Mpa/38mm mass concrete strip footing in a position as directed by the Representative/Agent and including demolishing and removal after completion of all brickwork.","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TOTAL MASONRY",{"$nulls":3},{"$f":"SUM(E1533:E1701)","v":{"v":0,"d":"0.00"}}]
[null,null,0,null,{"v":0,"d":"R0.00"}]
["SECTION 2","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NEW HOSPITAL ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["BILL NO 4","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["WATERPROOFING","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PREAMBLES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Preambles for Trades as defined in Scope of Work (C3.1 Item 4.1 & Item 4.2)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TRADE NAMES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Any reference to trade names in the Bills of Quantities or  Architect's specification or drawings shall deem to mean \"or similar and approved\"",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 120 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["DAMP-PROOFING OF WALLS AND FLOORS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["One layer of 375 micron black embossed polyethylene damp-proof course, with 200mm overlap at end laps & corners. ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["In walls","m2",7374,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Under sills, around windows, etc.","m2",1849,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["One layer of 250 micron green polyethylene waterproof sheeting sealed at laps with PVC self adhesive tape","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Under surface beds","m2",44142,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["WATERPROOFING TO ROOFS ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sikatop seal - 107 ZA waterproofing membrane installed in accordance with the manufacturer`s specifications. (Sika 051 430 0333) as per detail drawing HDG - TYP-042-008 & TYP-042-010 or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On parapet walls","m2",340,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Horizontally to top of concrete upstand ","m2",813,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Vertically to concrete upstand ","m2",530,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sikalastic®-560 waterproofing membrane installed in accordance with the manufacturer`s specifications. (Sika 051 430 0333) or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On flat roofs to falls","m2",13190,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Vertically to concrete upstand ","m2",2242,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but circular on plan","m2",19,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Horizontally to top of concrete upstand ","m2",33,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but circular on plan","m2",14,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Additional membrane 300mm girth at internal and external angles","m",14947,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D1757*C1757","v":{"v":0,"d":"R0.00"}}]
["Additional membrane 300mm girth at internal and external angles circular on plan","m",127,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Dressing and sealing into 110mm internal diameter fullbore outlet, including additional membrane","No",278,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Flood tests and guarantees","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for carrying out flood test to all areas","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Provide 10 year guarantee in accordance to manufacturer's specification effective from Date of Practical Completion ","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Prime all surfaces to be waterproofed with Pro-Struct 201 Bituminous Primer, including all verges and around outlets and protrusions, then allow the solvent to flash off. Extremely porous surfaces should be re-primed. Apply a 300mm wide gusset strip of Deltaplast Plain 3mm thick centrally at all floor screed and wall junctions. Dress all full-bore outlets with a single layer of 3mm thick Deltaplast Plain. Seal the entire full-bore outlet with Pro-Struct 203 Rubberised Bitumen Emulsion Reinforced with Pro-Struct 200 reinforced membrane (as per the Technical Data Sheet of Pro-Struct 203). Apply a single layer of Deltaplast TNT Mineral, reinforced with 180g/m² non-woven polyester membrane, weighing 4.5kg/m². Fully bond the membrane, by heat fusion, onto the primed area. Side laps of 75mm shall be carefully sealed by heat fusion, allowing a small bead of molten Bitumen to become visible at the exposed edge of the sheet. Seal these edges with a roller while the Bitumen is still in a molten state or similar approved. All in accordance to manufacturers specification ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On flat roofs to falls","m2",5334,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Vertically to concrete upstand ","m2",117,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Horizontally to top of concrete upstand ","m2",58,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Additional membrane 300mm girth at internal and external angles","m",1168,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Flood tests and guarantees","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for carrying out flood test to all areas","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Provide 10 year guarantee in accordance to manufacturer's specification effective from Date of Practical Completion ","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PROTECTIVE ROOFING PAINT ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Two coats 'Roofcote' bituminous aluminium paint or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On waterproofing to roofs including turn-ups and turn-downs ","m2",15498,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TOTAL WATERPROOFING",{"$nulls":3},{"$f":"SUM(E1703:E1789)","v":{"v":0,"d":"0.00"}}]
[null,null,0,null,{"v":0,"d":"R0.00"}]
["SECTION 2","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NEW HOSPITAL ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["BILL NO 5","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["ROOF COVERINGS, CLADDINGS, ETC","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PREAMBLES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Preambles for Trades as defined in Scope of Work (C3.1 Item 4.1 & Item 4.2)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TRADE NAMES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Any reference to trade names in the Bills of Quantities or  Architect's specification or drawings shall deem to mean \"or similar and approved\"",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Guarantees","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The roof covering and cladding is to be carried out strictly in accordance with the manufacturer's instruction. On completion the roof covering and accessories are to be inspected by the Manufacturer who is to provide a 5 year guarantee against defective materials and faulty workmanship  The roof is to be guaranteed weather tight for a period of 12 month period, calculated from the handed over date of the completed project",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 124 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PROFILED METAL SHEETING AND ACCESSORIES ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["0.53mm thick Global Roofing Solutions 700mm cover Klip-Tite™ profile Colorbond® Ultra Steel AZ200 spleter colour coated finish to top side - Colour: (Non standard colour to Architect's approval) and (Non standard colour to Architect's approval) backing coat roof sheeting, fixed to steel intermediate purlins at Max 2300mm centres and eaves and ridge purlins at Max 1900mm centres using KL700 clips, U-spacers to suit and sheet metal bearing strips of 150mm x 0.8mm thick over insulation fixed with 10No.16 x 16mm long self drilling wafer head PH2 screws or similar approved. All in accordance with the manufacturer`s specifications.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Roof sheeting with pitch not exceeding 25 degrees, fixed to steel purlins fixed concurrent with 40mm lambdaboard (measured elsewhere) ","m2",21876,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Roof sheeting with pitch not exceeding 25 degrees, fixed to steel purlins fixed concurrent with 70mm lambdaboard (measured elsewhere) ","m2",144,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D1821*C1821","v":{"v":0,"d":"R0.00"}}]
["Roof sheeting with pitch not exceeding 25 degrees, fixed to steel purlins fixed concurrent with 80mm lambdaboard (measured elsewhere) ","m2",5454,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Side cladding, fixed to steel purlins with additional screws to cladding rails fixed concurrent with 40mm lambdaboard (measured elsewhere) ","m2",2662,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Eave closures, fixed to steel purlins","m2",125,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["0.53mm Thick flashings shall be manufactured from Colorbond® Ultra Steel AZ200 spleter colour coated finish to top side - Colour: (Non standard colour to Architect's approval) and (Non standard colour to Architect's approval) backing coat, fixed to steel purlins (measured elsewhere) by way of S10 brackets or similar approved. All in strict accordance with manufacturer's specification. Colours and type to Architect’s approval","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["External corner flashing (Code FK72), 616mm girth, three times bent along girth and notched on site to suit roof profile. Complete with metal and poly closers ","m",562,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ridge capping (Code FK73) girth 550mm, three times bent along girth and notched on site to suit profile. Complete with metal and poly closers","m",1333,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Barge flashing (Code FK74) girth 550mm, three times bent along girth and notched on site to suit roof profile. Complete with metal and poly closers","m",1405,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Drip flashing (Code: FK76) 231mm girth three times bent along girth and notched on site to suit roof profile. Complete with metal and poly closers ","m",562,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Side wall flashing (Code FK79) 408mm girth, two times bent along girth, Counter flashing (Code FK77) 185mm girth, two times bent along girth. Complete with metal and poly closers","m",94,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Apex flashing girth 550mm, three times bent along length and notched on site to suit roof profile. Complete with metal and poly closers","m",245,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["4mm Aluminium composite material cladding, PC amount of Two Thousand Rand (R 2 000-00) nett, installed complete. The whole to be designed and installed by approved specialist, all in accordance with the manufacturer`s recommendations. ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Side cladding fixed to steel purlins","m2",75,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["2mm Thick galvanised steel flashings over movement joints as per detail drawing HDG - TYP-042-009","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Galvanised steel flashing 650mm girth, three times bent along length, plugged to both sides to concrete or brickwork ","m",46,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["RAINWATER DISPOSAL","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Purpose made 0.53mm thick galvanized gutter bend into profile, including matching rivet-fixed mitres and end caps internally sealed using an approved soft sealant, hung by nail fixed internal aluminium hangers at 800mm centres with rectangular fluted downpipes. Complete with rainwater spouts as per type and size all to detail drawings. Bolted together with galvanized bolts (sealed watertight with an approved soft sealant), with min 500mm overlaps. Shop drawings and sample to be approved by Architect prior to bulk manufacturing. Colours (Non-standard) to Architect’s approval.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150 x 100mm Eaves gutters to falls, with front edge, on and including gutter brackets fixed to steel roofs","m",71,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150 x 150mm Eaves gutters to falls, with front edge, on and including gutter brackets fixed to steel roofs","m",1172,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150 x 200mm Eaves gutters to falls, with front edge, on and including gutter brackets fixed to steel roofs","m",900,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over 150 x 100mm eaves gutter for stopped end","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over 150 x 150mm eaves gutter for stopped end","No",146,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over 150 x 200mm eaves gutter for stopped end","No",60,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over eaves gutter for outlet with nozzle for 100 x 75mm pipe ","No",232,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100 x 75 mm Rainwater downpipes, fixed to walls with pre-painted downpipe cleats using nail-in anchor fixings","m",1858,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra for eaves offset, 300mm projection","No",45,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra for eaves offset, 1050mm projection","No",14,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over for shoe","No",232,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Purpose made 2mm thick galvanized gutter bend into profile, including matching rivet-fixed mitres and end caps internally sealed using an approved soft sealant, hung by nail fixed internal aluminium hangers at 800mm centres with rectangular fluted downpipes. Complete with rainwater spouts as per type and size all to detail drawings. Bolted together with galvanized bolts (sealed watertight with an approved soft sealant), with min 500mm overlaps. Shop drawings and sample to be approved by Architect prior to bulk manufacturing. Colours (Non-standard) to Architect’s approval.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["500 x 300mm Eaves gutters to falls, with front edge, on and including gutter brackets fixed to steel roofs","m",200,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over 500 x 300mm eaves gutter for stopped end","No",10,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over eaves gutter for outlet with nozzle for 100 x 75mm pipe ","No",10,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["ROOF AND WALL INSULATION","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D1885*C1885","v":{"v":0,"d":"R0.00"}}]
["40mm Lambdaboard density 34kg/m³ closed cell Polyisocyanurate insulation with White mineral facing to one side, fixed concurrent with roof covering over purlins with aluminium T section fixed at 1200mm centres or similar approved. All in accordance with the manufacturer's recommendations, complete with SABISA certificate.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Insulation laid over purlins fixed concurrent with roof covering ","m2",21876,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["40mm Lambdaboard density 34kg/m³ laminated Polyisocyanurate with White mineral facing on one side and mineral natural on the other, fixed to the vertical frame work of the purlins. System to be mechanically fastened as per manufacturer’s instruction or similar approved. All in accordance with the manufacturer's recommendations, complete with SABISA certificate.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Insulation laid vertical over cladding rails fixed concurrent with side cladding ","m2",2662,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["70mm Lambdaboard density 34kg/m³ laminated Polyisocyanurate with White mineral and mineral white facing on one side and mineral natural on the other, fixed to battens 900mm centres. System to be mechanically fastened as per manufacturer’s instruction or similar approved. All in accordance with the manufacturer's recommendations, complete with SABISA certificate.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Insulation laid between purlins fixed concurrent with roof covering ","m2",144,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["80mm Lambdaboard density 35kg/m³ closed cell Polyisocyanurate insulation with White mineral facing to one side, fixed concurrent with roof covering under purlins with \"H\" bar joiners screw fixed at 1200mm centres with 5mm gap between boards butt-joined over purlins or similar approved. All in accordance with the manufacturer's recommendations, complete with SABISA certificate.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Insulation laid under purlins fixed concurrent with roof covering ","m2",5454,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["ROOF COVERINGS, CLADDINGS, ETC",{"$nulls":3},{"$f":"SUM(E1791:E1901)","v":{"v":0,"d":"0.00"}}]
[null,null,0,null,{"v":0,"d":"R0.00"}]
["SECTION 2","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NEW HOSPITAL ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["BILL NO 6","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["CARPENTRY AND JOINERY","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PREAMBLES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Preambles for Trades as defined in Scope of Work (C3.1 Item 4.1 & Item 4.2)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TRADE NAMES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Any reference to trade names in the Bills of Quantities or  Architect's specification or drawings shall deem to mean \"or similar and approved\"",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SUPPLEMENTARY PREAMBLES","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Descriptions","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The term \"planted on\" shall mean the nailing of one timber member to another  The term \"screwed on\" shall mean the countersunk screwing of one timber member to another",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The term \"screwed on and pelleted\" shall mean the screwing of one timber member to another with the heads of screws sunk and pelleted  The term \"plugged\" shall mean the countersunk screwing of a timber member to and including plastic plugs in brickwork or concrete ",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The term \"plugged and pelleted\" shall mean the screwing of a timber member to and including plastic plugs in brickwork or concrete with heads of screws sunk and pelleted  Shelving, etc. described as screwed to steel must be fixed from underside and prices are to include for countersunk drilling through the steel for screw fixing  Descriptions of floors, ceilings, joinery, etc. shall be deemed to include for all square cutting  Descriptions of items given in lineal metre shall be deemed to include for mitres, stopped ends, fitted intersections, etc . Descriptions of rounded angles, rebates, grooves, chamfers, moulded edges, etc. shall be deemed to include for angles, ends, etc.",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Timber","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["All softwood to be South African Pine ____________________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 126 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["DOORS, ETC.","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["44mm Weatherboard flush door with vertical tongue and groove hardwood back to back boarding on both sides","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Single door size 813 x 1738mm high","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Double door 1800 x 2032mm high in two equal leaves","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["40mm Semi-solid core flush panel door with masonite finish both sides with hardwood concealed edge strip fitted with lock block to one edge","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Single door size 505 x 1738mm high","No",23,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Single door size 762 x 1738mm high","No",14,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D1949*C1949","v":{"v":0,"d":"R0.00"}}]
["Single door size 813 x 1738mm high","No",214,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Single door size 813 x 1882mm high ","No",273,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Single door size 813 x 2032mm high","No",167,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Single door size 956 x 1882mm high","No",29,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Single door size 956 x 2032mm high","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Single door size 965 x 2032mm high","No",1146,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Single door size 956 x 2032mm high with 250 x 631mm high opening for glass view panel in aluminium frame (glass elsewhere)","No",147,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Single door size 980 x 1565mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Single door size 1264 x 2032mm high","No",11,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Single swing double door 1800 x 2032mm high in two equal leaves","No",28,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Double door 986 x 1738mm high in two equal leaves","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Double door 1436 x 1738mm high in two equal leaves","No",65,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Double door 1350 x 2032mm high in two unequal leaves, 900mm and 450mm wide respectively","No",57,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Double door 1350 x 2032mm high in two unequal leaves, 900mm and 450mm wide respectively and one leaf with 250 x 631mm high opening for glass view panel in aluminium frame (glass elsewhere)","No",181,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Double door 1500 x 2032mm high in two unequal leaves, 900mm and 600mm wide respectively","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Double door 1510 x 2032mm high in two equal leaves, each with 250 x 631mm high opening for glass view panel in aluminium frame (glass elsewhere)","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Double door 1588 x 2032mm high in two equal leaves","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Double door 1800 x 2032mm high in two equal leaves, each with 250 x 631mm high opening for glass view panel in aluminium frame (glass elsewhere)","No",127,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Double sliding door 2000 x 2032mm high in two equal leaves each with one 250 x 631mm high opening for glass view panel in aluminium frame (glass elsewhere)","No",19,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Double sliding door 1950 x 2108mm high in two equal leaves each with one 250 x 631mm high and one 250 x 400mm high opening for glass view panel in aluminium frame (glass elsewhere)","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["44mm Solid core flush panel door with masonite finish both sides with hardwood concealed edge strip fitted with lock block to one edge","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Double swing single door 965 x 2032mm high with 250 x 631mm high opening for glass view panel in aluminium frame (glass elsewhere)","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Double swing single door 1036 x 2032mm high with 250 x 631mm high opening for glass view panel in aluminium frame (glass elsewhere)","No",46,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sliding door 952 x 2100mm high with one 250 x 631mm high opening for glass view panel in aluminium frame (glass elsewhere)","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sliding door 1172 x 2100mm high with one 250 x 631mm high opening for glass view panel in aluminium frame (glass elsewhere)","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sliding door 1352 x 2100mm high with one 250 x 631mm high opening for glass view panel in aluminium frame (glass elsewhere)","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sliding door 1652 x 2100mm high with one 250 x 631mm high opening for glass view panel in aluminium frame (glass elsewhere)","No",16,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sliding door 1952 x 2100mm high with one 250 x 631mm high opening for glass view panel in aluminium frame (glass elsewhere)","No",9,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Pelican MIS Systems lead lined X ray type doors with 2mm thick lead lining and sapele veneer both sides or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["48mm Single door 957 x 2032mm high ","No",15,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["48mm Double door 1350 x 2032mm high in two unequal leaves, 900mm and 450mm wide respectively","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["48mm Sliding door 1352 x 2100mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D2013*C2013","v":{"v":0,"d":"R0.00"}}]
["48mm Sliding door 1952 x 2100mm high ","No",11,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Pelican Mis Systems Pyropanel Class D 120 minute fire door with 120 isolation and with 3,6mm treated commercial ply on both sides including intumescent strip to top of door and with concealed edge strips all round including 2,0mm pressed steel frames suitable for half brick walls and preparing frame for door closer and lock or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["61mm Single leaf door 686 x 1738mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["61mm Single leaf door 813 x 2065mm high","No",7,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["61mm Single leaf door 965 x 2065mm high","No",9,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["61mm Single leaf door 1000 x 2065mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["61mm Double door 1350 x 2032mm high in two unequal leaves, 900mm and 450mm wide respectively","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["61mm Double door 1436 x 1738mm high with two equal leaves","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["61mm Double door 1588 x 2065mm high with two equal leaves","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["61mm Double door 1736 x 2065mm high with two equal leaves","No",12,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Pelican Mis Systems Pyropanel Class D 120 minute fire door with 120 isolation and with 3,6mm treated commercial ply on both sides including intumescent strip to top of door and with concealed edge strips all round including 2,0mm pressed steel frames suitable for one brick walls and preparing frame for door closer and lock or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["61mm Single leaf door 686 x 1738mm high","No",10,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["61mm Single leaf door 686 x 2065mm high","No",8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["61mm Single leaf door 762 x 2065mm high","No",14,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["61mm Single leaf door 813 x 1738mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["61mm Single leaf door 813 x 2065mm high","No",12,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["61mm Single leaf door 965 x 2065mm high","No",48,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["61mm Single leaf door 1000 x 2065mm high","No",91,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["61mm Double door 1350 x 2032mm high in two unequal leaves, 900mm and 450mm wide respectively","No",10,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["61mm Double door 1436 x 1738mm high with two equal leaves","No",32,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["61mm Double door 1588 x 2065mm high with two equal leaves","No",72,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["61mm Double door 1736 x 2065mm high with two equal leaves","No",234,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["61mm Double door 2000 x 2065mm high with two equal leaves","No",14,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Pelican Mis Systems lead lined X ray type Pyropanel Class D 120 minute fire door with 2mm thick lead lining, 120 isolation and 3,6mm treated commercial ply on both sides including intumescent strip to top of door and with concealed edge strips all round including 2,0mm pressed steel frames suitable for one brick walls and preparing frame for door closer and lock or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["61mm Double door 1736 x 2065mm high with two equal leaves","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Maxiflex flexible clear plastic PVC impact traffic double door (Colour: Ivory White) made of 7mm thick transparent PVC sheets, including PVC bumpers, Maxiflex corrosion free galvanised steel section frame mounted to sub-frame, with concealed double action torsion spring closers or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Double door 1200 x 2032mm high in two equal leaves","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SKIRTING","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Hardwood skirting","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["19 x 75mm Skirting plugged","m",1793,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["19 x 75mm Skirting stepped over treads and risers of stairs, plugged","m",73,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["CORNICE ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D2077*C2077","v":{"v":0,"d":"R0.00"}}]
["Hardwood Cornice","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["46mm x 24mm Hardwood Cornice, complete with 10mm x 10mm shadow-line at sidewall and splayed corner at internal face ","m",4195,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["COUNTERS, CUPBOARD AND WORK TOPS ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following counters and cupboards have been measured as complete units i.e. the components of the units have not been separately measured. The descriptions, therefore, of such units shall be deemed to include all components, assembling, housing, notching, glueing, blocking, planting on and screwing with countersunk screws, edge strips, decorative plastic finish, glass, ironmongery, metalwork, etc. Tops have been measured separately unless otherwise described)",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: All work tops shall be sealed against walls, around basins, sinks, etc. with an approved type non-fungal sustaining clear silicone sealant",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["General carcass material specification","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Unless otherwise specified, carcass construction of furniture components to be bison board V313 moisture resistant particle board in accordance with SANS EN 312:1997 or Supawood medium density fibreboard (MDF) SANS 540-1:1991, melamine surfaced to both faces Bisonlam melamine faced board in accordance with SANS 1763:1998, finish in minimum 2mm thickness pvc edging",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["General door material specification","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Unless otherwise specified door and drawer frontals to be form Bisonbord V313 high moisture resistant particle board in accordance with SANS EN 312:1997 or Supawood medium density fibreboard (MDF) SANS 540-1:1991 surface in 0.8mm formica high pressure laminate (HPL) in accordance with SANS ISO 4586:1995 CL grade white liner to inner faces",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["General worktop material specification","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Unless otherwise specified all worktops fitted to walls of fitted to cupboards and cabinets to be form Bisonbord v 313 high moisture resistant particle board in accordance with SANS EN 312-5:1997 moisture resistant particle board with profiled edges, Surface in formica high pressure laminate in accordance with SANS ISO 4586:1995 to upper faces and with formica high pressure laminate in accordance with SANS ISO 4586:1995 brown backer balancer to reversed faces. All worktops butting up against walls to be edged in formica high pressure laminate in accordance with SANS ISO 4586:1995 and exposed edges finished in minimum 3mm pvc edging to required widths. All worktops against tiles to receive coved tile trims (genesis flexi-bead pvc coat sfb 061/01) butting up against worktop and tile surfaces.  Worktops fitted independently to walls generally fixed by means of mild steel wall cleats and support brackets with powder coated finished wall cleat and support brackets.  Colour of worktops: PG Bison C-Choice range",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["General counter top material specification","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Unless otherwise specified counter tops forming part of workstations and counters to be from Surinno solid surfacing material incorporating down stands profiled edges and up stands to design exhibiting seamless jointing. Apply onto Supawood medium density fibre board in accordance with SANS 540-1:1991 support structures",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["General vanity top material specification","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Unless otherwise specified vanity tops to be from Surinno solid surfacing material incorporate down stands profiled edges fitted up stands and cut-outs for moulded Surinno bowls and basins to design exhibiting seamless jointing. Apply onto Supawood medium density fibreboard in accordance with SANS 540-1:1991 support structures. Vanity tops fitted independently to walls generally fixed by means of mild steel wall cleats and support brackets with powder coated finish. Support brackets to be fitted at centres not exceeding 500mm.",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Wall cupboards - fixing to walls","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cupboard suspended from walls to be back mounted by means of cupboard suspension fittings fitted to cupboard side panels. Cupboards resting on floors to be screw and plugged, mounted to rear walls through cupboard top and bottom rear bearers fitted behind melamatched - 3mm Supawood colour matched to Melawood in-fill panels  Colour of cupboards: PG Bison D-Design range",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Skirting finishing to floors","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cupboards with skirting finished to front and side of components to be installed to prevent water seapage. Cupboard base structure front panel from Bisonbord V 313 high moisture resistant particle board in accordance with SANS EN 312-5:1997 to be embedded in a bed of silicone solution. Mounting of 0.8mm thick Formica high pressure laminate in accordance with SANS ISO 4586:1995 horizontal general purpose standard skirt panel to be silicone fitted to base structure behind.",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Product Standards","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["1: FORMICA HPL (High Pressure Laminate) in accordance with SANS ISO 4586:1995 2: FORMICA Solid Core HPL (High Pressure Laminate) in accordance with SANS ISO 4586:1995 3: FORMICA Solid Core HPL - Writing Surface (White Writing Surface and Green Chalkboard) in accordance with CKS 36:2004 and SANS ISO 4586:1995 4: DECCON CPL (Continuous Pressed Laminate) in accordance with SANS 1762:1998 5: MELAWOOD MFB (MELAMINE Faced Board) in accordance with SANS 1763:1998 6: BISONLAM MFB (MELAMINE Faced Board) in accordance with SANS 1763:1998 7: SUPALAM MFB (MELAMINE Faced Board) in accordance with SANS 1763:1998 8: BISONBORD Particleboard in accordance with SANS EN 312-3:1996 9: Bisonbord V 313 (High Moisture Resistant) Particleboard in accordance with SANS EN 312-5:1997 10: SUPAWOOD MDF (Medium Density Fibreboard) in accordance with SANS 540-1:1991 11: Door/drawer postformed 900 profile on two long edges and finished in a minimum 2mm thick PVC edging (colour as per Colour Schedule) on two short edges 12: FORMICA Life Seal worktop wit 32mm Bisonbord HMR substrate, 0.8mm FORMICA HPL - HG/P surface and 0.8mm FORMICA HPL - BK brown backer",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Product Types","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["A - Horizontal General Purpose/Standard - HG/S B - Horizontal General Purpose/Postform - HG/P C - Vertical General Purpose/Standard - VG/S D - Vertical General Purpose/Postform - VG/P E - Cabinet Liner - CL F - Brown Backer - BK",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sample furniture","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Architect may call upon sample furniture in order to evaluate quality and construction methods of joinery work.",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Door hinges","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["To be boss type hinges for side panel mounting, including trim cups. Install minimum 2 hinges per leaf up to 1000mm high and maximum 600mm spacing for hinges on doors higher than 1000mm.\nGrass type:\nTwist Lock - Code 218835 - 4903/165 degrees\nBacking Plate - Code 310765 - 4,3 / 6,5 Cross Plate\nEuro Screws - Code 483545 - 6 x 13 - 1 pair",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Drawer runners","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["To be full metal sided and rear - full retractable with 16mm Supalam melamine faced board in accordance with SANS 1763:1998 (colour: white) drawer bases Metalbox type Full extension (white) Reference Sides 500mm deep x 150mm high Reference Rear 150mm high 565.75.745",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sliding tray runners","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["To be full extension type, side mounted, soft roller\nHafele type\nLength 350mm, extension length 375mm\nReference: 420.76.362",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Door locks (All doors and drawers to be lockable - keyed alike per room with Master key per Department)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D2141*C2141","v":{"v":0,"d":"R0.00"}}]
["To be from Cyberlock, short bolt travel left or right (Finish : Nickel Plates)SDT/GRASS REF: Rim Lock Nickle 22mm (Mastered) 7CL601-22-N MOUNTING SCREWS: 746190 - 6x19 screws",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Pigeon hole door locks","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Pigeon hole special locks to be suitable for use of padlocks.\nHafele Type\nLevel lock, zinc alloy, polished chrome, with left or right\nhand locking travel\nReference A-right 235.61.200\nReference B-Left 236.61.201",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Drawer locks (Linked to Master Key System)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Drawers to be locked in series of four in height, with face fitting Cyberlock Central Locking system for recessing in the cabinet side panel  SDT/GRASS REF: 700mm Central Locking System/Nickle (4 Drawer) 7CL603-700-N ",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Carcass Connectors","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["For factory machined ready to assemble purpose\nBlum Type Knock-down\nReference 42/070",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Shelf supports","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["For factory machined ready to assemble purposes\nBlum Type\nNylon Housing Ref 40.4001\nNylon Cover Cap Ref 41.5400\nFinishing Screw Ref 636.1050\nNylon Bush Ref 41.1100",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cupboard door catches","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Buchel Type Elbow catch (rooster)\nReference B1566",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Door stops","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Hafele Type Press fit White\nReference 356.20.725",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Worktop connectors","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Hafele Type\nSuitable for 32mm built-up Formica tops Minimum three\nper 45° full joints\nReference 262.96.211\nUsed in conjunction with Lamello joint pieces",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Broomstick holders","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["For four holders per broom cupboard\nHafele Type\nReference 520.10.009",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Distribution Cupboards - Pressure Catches","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Type Hafele - automatic spring catch to each door\nReference 245.54.701",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cabinet suspension fittings","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Hafele Type\nReference Left-290.01.701\nReference Right-290.02.700\nSuspension rail\nReference 290.02.900",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Handles (To all doors and drawers)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Hafele Type\nReference 129.57.701 (Colour as per Colour\nSchedule)",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ventilation grilles (To all CPU cupboards)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Six ventilation grills - finish plastic, chrome plated.\nHafele Type Reference 571.54.220",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Wardrobe rail (full length of cupboard hang space)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Length x 25mm Nickel plated polished wardrobe rail.\nHafele Type Reference 801.11.741\nTwo rail end support per rail Nickel plated.\nHafele Type Reference 803.51.757",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["FLOOR CUPBOARDS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["450 x 560 x 880mm High floor cupboard complete (See Drawing 045-CUPF001 attached to the back of these bills of quantities) and as per 100-M-Joinery schedule from HDG","No",27,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["450 x 560 x 880mm High floor drawer cupboard complete (See Drawing 045-CUPF003 attached to the back of these bills of quantities) and as per 100-M-Joinery schedule from HDG","No",298,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["900 x 560 x 880mm High floor cupboard complete (See Drawing 045-CUPF004 attached to the back of these bills of quantities) and as per 100-M-Joinery schedule from HDG","No",421,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["1000 x 560 x 880mm High floor cupboard complete (See Drawing 045-CUPF005 attached to the back of these bills of quantities) and as per 100-M-Joinery schedule from HDG","No",71,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D2205*C2205","v":{"v":0,"d":"R0.00"}}]
["900 x 900 x 880mm High corner floor cupboard complete (See Drawing 045-CUPF006 attached to the back of these bills of quantities) and as per 100-M-Joinery schedule from HDG","No",32,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["450 x 600 x 2040mm High broom cupboard (left hand) complete (See Drawing 045-CUPF007 attached to the back of these bills of quantities) and as per 100-M-Joinery schedule from HDG","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["900 x 560 x 2040mm High utility floor cupboard complete (See Drawing 045-CUPF008 attached to the back of these bills of quantities) and as per 100-M-Joinery schedule from HDG ","No",32,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["900 x 600 x 2040mm High linen cupboard complete (See Drawing 045-CUPF012 attached to the back of these bills of quantities) and as per 100-M-Joinery schedule from HDG","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["450 x 560 x 718mm High counter floor cupboard (left) complete (See Drawing 045-CUPF016 attached to the back of these bills of quantities) and as per 100-M-Joinery schedule from HDG","No",425,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["1000 x 560 x 2040mm High built-in cupboard complete (See Drawing 045-CUPF020 attached to the back of these bills of quantities) and as per 100-M-Joinery schedule from HDG.","No",14,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["450 x 560 x 718mm High counter floor drawer cupboard complete (See Drawing 045-CUPF022 attached to the back of these bills of quantities) and as per 100-M-Joinery schedule from HDG","No",435,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["300 x 560 x 718mm High CPC floor cupboard (left) complete (See Drawing 045-CUPF026 attached to the back of these bills of quantities) and as per 100-M-Joinery schedule from HDG","No",10,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["450 x 560 x 2040mm High grocery floor cupboard (left) complete (See Drawing 045-CUPF034 attached to the back of these bills of quantities) and as per 100-M-Joinery schedule from HDG","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["750 x 350 x 900mm High floor linen cupboard (double doors equal size) (See Drawing 045-CUPF052 attached to the back of these bills of quantities) and as per 100-M-Joinery schedule from HDG ","No",12,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["900 x 560 x 718mm High floor linen cupboard (double doors equal size) (See Drawing 045-CUPF053 attached to the back of these bills of quantities) and as per 100-M-Joinery schedule from HDG","No",30,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["900 x 560 x 2200mm High floor cupboard (double doors equal size) (See Drawing 045-CUPF064 attached to the back of these bills of quantities) and as per 100-M-Joinery schedule from HDG","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["900 x 560 x 649mm High laboratory floor cupboard on castors complete (See Drawing 045-CUPF065 attached to the back of these bills of quantities) and as per 100-M-Joinery schedule from HDG","No",18,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["1000 x 560 x 880mm High specialist dental drawer unit complete (See Drawing 045-CUPF089 attached to the back of these bills of quantities) and as per 100-M-Joinery schedule from HDG","No",20,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["500 x 500 x 2000mm High bedside floor cupboard (single door including drawer and shelving) (See Drawing 045-CUPF103 attached to the back of these bills of quantities) and as per 100-M-Joinery schedule from HDG","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["900 x 600 x 2040mm High combination floor cupboard and filing cabinet (double doors equal size)  (See Drawing 045-CUPF104 attached to the back of these bills of quantities) and as per 100-M-Joinery schedule from HDG","No",303,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["900 x 450 x 880mm High floor cupboard (double doors equal size) (See Drawing 045-CUPF108 attached to the back of these bills of quantities) and as per 100-M-Joinery schedule from HDG","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["450 x 450 x 880mm High floor drawer cupboard (four pull-out drawers equal in height) (See Drawing 045-CUPF109 attached to the back of these bills of quantities) and as per 100-M-Joinery schedule from HDG","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["FLOOR CUPBOARDS IN-FILL PANELS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Floor cupboard infill panels to one or two end for cupboards in length where wall dimensions are greater than cupboards (See Drawing 045-CUPF018 attached to the back of these bills of quantities) and as per 100-M-Joinery schedule from HDG","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["WALL CUPBOARDS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["450 x 300 x 720mm High wall cupboard complete (See Drawing 045-CUPW001 attached to the back of these bills of quantities) and as per 100-M-Joinery schedule from HDG","No",24,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["900 x 300 x 720mm High wall cupboard complete (See Drawing 045-CUPW003 attached to the back of these bills of quantities) and as per 100-M-Joinery schedule from HDG","No",148,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["1000 x 300 x 720mm High wall cupboard complete (See Drawing 045-CUPW004 attached to the back of these bills of quantities) and as per 100-M-Joinery schedule from HDG","No",161,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["711 x 300 x 711mm High wall cupboard drug cabinet type D - W06 complete (See Drawing 045-CUPW006 attached to the back of these bills of quantities) and as per 100-M-Joinery schedule from HDG","No",9,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["650 x 450 x 800mm High microwave wall cupboard complete (See Drawing 045-CUPW016 attached to the back of these bills of quantities) ","No",87,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["450 x 300 x 720mm High wall cupboard (without doors) complete (See Drawing 045-CUPW020 attached to the back of these bills of quantities) and as per 100-M-Joinery schedule from HDG","No",21,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["900 x 300 x 720mm High wall cupboard (without doors) complete (See Drawing 045-CUPW022 attached to the back of these bills of quantities) and as per 100-M-Joinery schedule from HDG","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["1000 x 300 x 720mm High wall cupboard (without doors) complete (See Drawing 045-CUPW023 attached to the back of these bills of quantities) ","No",7,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PIGEON HOLES","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["750 x 350 x 2040mm High pigeon hole cupboard complete (See Drawing 045-CUPF013 attached to the back of these bills of quantities) ","No",73,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["600 x 350 x 600mm High pigeon hole cupboard complete (See Drawing 045-CUPW035 attached to the back of these bills of quantities) and as per 100-M-Joinery schedule from HDG","No",41,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D2269*C2269","v":{"v":0,"d":"R0.00"}}]
["500 x 711 x 1750mm High pigeon hole cupboard complete (See Drawing 045-CUPF032 attached to the back of these bills of quantities) and as per 100-M-Joinery schedule from HDG","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["400 x 350 x 2040mm High pigeon hole cupboard complete (See Drawing 045-CUPF057 attached to the back of these bills of quantities) ","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["DESKS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["1507 x 1827mm Overall size desk complete including  drawer cupboards, lever arch storage cupboard and pigeon hole storage cupboard to design (See Drawing 045-DES017) attached to the back of these bills of quantities) as per 100-M-Joinery schedule from HDG (DES017)","No",82,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["1507 x 1827mm Overall size desk complete including  drawer cupboards, lever arch storage cupboard and pigeon hole storage cupboard to design (See Drawing 045-DES018) attached to the back of these bills of quantities) as per 100-M-Joinery schedule from HDG (DES018)","No",11,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["FLOOR CUPBOARD TOPS ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Worktop from 32mm High Moisture Resistant Particleboard with 0.8mm HPL (High Pressure Laminate) HG/P surface including 0,8mm HPL (High Pressure Laminate) - BK backer to comply with SANS ISO 4586:1995 standards. All exposed ends of worktops edged in 3mm PVC edging (colour as Architect approval) to full profile and edges butting up against walls, cut-outs in worktop to accommodate sink, etc to size (sink, etc measured elsewhere). Cut-out edge to worktop to accommodate sink, etc to receive minimum two coats approved water repellent sealant.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["32mm Thick 90 degree post-formed top 600mm wide (See Drawing 045-T057-T060 attached to the back of these bills of quantities) and as per 100-M-Joinery schedule TOP057-060 (Total in no: 280)","m",850,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["32mm Thick 90 degree post-formed top 600mm wide circular on plan (See Drawing 045-T057-T060 attached to the back of these bills of quantities) and as per 100-M-Joinery schedule TOP057-060 (Total in no: 1)","m",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Worktop from 32mm High Moisture Resistant Particleboard with 0.8mm HPL (High Pressure Laminate) HG/P surface including 0,8mm HPL (High Pressure Laminate) - BK backer to comply with SANS ISO 4586:1995 standards. With and including a 90 degrees 16 x 100mm high post formed rear and side splash back where necessary to be supplied and installed separately. All exposed ends of worktops edged in 3mm PVC edging (colour as Architect approval) to full profile and edges butting up against walls, cut-outs in worktop to accommodate sink, etc to size (sink, etc measured elsewhere). Cut-out edge to worktop to accommodate sink, etc to receive minimum two coats approved water repellent sealant.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["32mm Thick 180 degree post-formed top 600mm wide (See Drawing 045-T01-T04 attached to the back of these bills of quantities) and as per 100-M-Joinery schedule TOP001-004 (Total in no: 496)","m",1447,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Hardwood 32mm top finished with an approved sealant to preserve wood. With and including 10 x 100mm high hardwood splash back plugged to walls rear and side splash back where necessary to be supplied and installed separately. Cut-outs in worktop to accommodate sink, etc to size (sink, etc measured elsewhere). Cut-out edge to worktop to accommodate sink, etc to receive minimum two coats approved water repellent sealant.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["32mm Thick hardwood top 700mm wide (See Drawing 045-T018 attached to the back of these bills of quantities) and as per 100-M-Joinery schedule TOP018 (Total in no: 16)","m",46,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Laminated saligna top with rounded front finished with an approved sealant to preserve wood. With and including 10 x 100mm high hardwood splash back plugged to walls rear and side splash back where necessary to be supplied and installed separately. ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["50mm Thick laminated saligna top 900mm wide (See Drawing 045-T022 attached to the back of these bills of quantities) and as per 100-M-Joinery schedule TOP022 (Total in no: 18)","m",34,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Worktops from 12mm thick solid surface material joined inconspicuously with matching adhesive and bonded to 16mm Medium Density Fibreboard (MDF) in accordance with SANS 540-1:1991 substrate with an approved silicone, fabricated and constructed by an approved fabricator, all in accordance with the manufacturer`s recommendations, to incorporate minimum 6mm radius corners in lengths, vanity unit with open ends to incorporate down stand/return to width of top","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["28mm Thick  90 degree post-formed top 600mm wide with 30mm high front edge (See Drawing 045-T017 attached to the back of these bills of quantities) and as per 100-M-Joinery schedule TOP017 (Total in no: 25)","m",65,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["WALL FITTED TOPS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Worktop from 32mm Medium Density Fibreboard with 0.8mm HPL (High Pressure Laminate) HG/P surface including 0,8mm HPL (High Pressure Laminate) - BK backer to comply with SANS ISO 4586:1995 standards, with and including downstand 32 x 200mm 90 degree post formed to one end. With and including a 90 degrees 16 x 100mm high post formed rear and side splash back where necessary to be supplied and installed separately. All exposed ends of worktops edged in 3mm PVC edging (colour as Architect approval) to full profile and edges butting up against walls, cut-outs in worktop to accommodate sink, etc to size (sink, etc measured elsewhere). Cut-out edge to worktop to accommodate sink, etc to receive minimum two coats approved water repellent sealant.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["32mm Thick 90 degree post-formed top 550mm wide (See Drawing 045-T005-T008 attached to the back of these bills of quantities) and as per 100-M-Joinery schedule TOP005-008 (Total in no: 61)","m",179,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Worktops including 200mm downstand, from 12mm thick solid surface material joined inconspicuously with matching adhesive and bonded to 16mm Medium Density Fibreboard (MDF) in accordance with SANS 540-1:1991 substrate with an approved silicone, fabricated and constructed by an approved fabricator, all in accordance with the manufacturer`s recommendations, to incorporate minimum 6mm radius corners in lengths, vanity unit with open ends to incorporate down stand/return to width of top, cut-outs in vanity units to receive under mounted hand wash basins, special bowls, etc (measured elsewhere) vanity units to exhibit seamless joints throughout. ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["28mm Thick top 550mm wide (See Drawing 045-T074 attached to the back of these bills of quantities) and as per 100-M-Joinery schedule TOP074-077 (Total in no: 21)","m",23,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["28mm Thick top 550mm wide (See Drawing 045-T075 attached to the back of these bills of quantities) and as per 100-M-Joinery schedule TOP074-077 (Total in no: 7)","m",13,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["28mm Thick top 550mm wide (See Drawing 045-T076 attached to the back of these bills of quantities) and as per 100-M-Joinery schedule TOP074-077 (Total in no: 3)","m",9,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["28mm Thick top 550mm wide (See Drawing 045-T077 attached to the back of these bills of quantities) and as per 100-M-Joinery schedule TOP074-077 (Total in no: 1)","m",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SUNDRIES","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Mild steel brackets","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Support brackets for tops weld to joints, pre-drilled and countersunk holed for wall and worktop fixings formed of 32 x 32 x 3.2mm thick mild steel square tube white power coated, size to Architect detail (See Drawing 045-S01-S04 attached to the back of these bills of quantities) and as per 100-M-Joinery schedule from HDG (SUP001)","No",2465,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Support brackets for tops weld to joints, pre-drilled and countersunk holed for wall and worktop fixings formed of 25 x 25 x 3mm thick mild steel square tube white power coated, size to Architect detail (See Drawing 045-S01-S04 attached to the back of these bills of quantities) and as per 100-M-Joinery schedule from HDG (SUP004)","No",79,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Support brackets for tops weld to joints, pre-drilled and countersunk holed for wall and worktop fixings formed of 25 x 25 x 3mm thick mild steel square tube white power coated, size to Architect detail (See Drawing 045-S01-S04 attached to the back of these bills of quantities) and as per 100-M-Joinery schedule from HDG (SUP019)","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Support brackets for tops weld to joints, pre-drilled and countersunk holed for wall and worktop fixings formed of 25 x 25 x 3mm thick mild steel square tube white power coated, size to Architect detail (See Drawing 045-S01-S04 attached to the back of these bills of quantities) and as per 100-M-Joinery schedule from HDG (SUP022)","No",76,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NURSES COUNTERS AND RECEPTION COUNTERS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D2333*C2333","v":{"v":0,"d":"R0.00"}}]
["Counter combination consisting of 12mm “Fenix NTM” (or similar approved) double sided matched colour core (colour to Architect approval) applied to a 20mm Supawood substrate including 100 vertical trim consisting of 1.2mm Fenix NTM (or similar approved) colour matched core applied to a 16mm Supawood substrate including 0.9mm Fenix NTM standard laminate (or similar approved) applied to the 20mm Supawood substrate. Outer counter vertical decorative face to receive 0.9mm Fenix NTM Standard Laminate applied to a 20mm Supawood substrate. Decorative 100 horizontal trim consisting of 1.2mm Fenix NTM (or similar) colour matched core applied to a 16mm Supawood substrate, joint to be seamless to worktop surfaces. Aluminium sheet skirting panel, bonded with adhesive to 16mm Supawood skirting panel to full length of counter and return.  Design inlay to be confirmed. Refer to the following typical detail drawings 045-C001, 045-C503, 045-C001-01, 045-001-02, 045-C419, 045-C420, 045-C501, 045-C503, 045-C504, 045-C505, 045-C506, 045-C507 attached to the back of these bills of quantities in conjunction with the drawings mentioned below.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 001 - BLOCK A LG COUNTER 001 complete (See Drawing A-045-C001 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 002 - BLOCK A LG COUNTER 002 complete (See Drawing A-045-C002 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 005 - BLOCK A LG COUNTER 005 complete (See Drawing A-045-C005 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 101 - BLOCK A GF COUNTER 101 complete (See Drawing A-045-C101 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 102 - BLOCK A GF COUNTER 102 complete (See Drawing A-045-C102 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 103 - BLOCK A GF COUNTER 103 complete (See Drawing A-045-C103 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 104 - BLOCK A GF COUNTER 104 complete (See Drawing A-045-C104 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 105 - BLOCK A GF COUNTER 105 complete (See Drawing A-045-C105 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 106 - BLOCK A GF COUNTER 106 complete (See Drawing A-045-C106 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 107 - BLOCK A GF COUNTER 107 complete (See Drawing A-045-C107 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 108 - BLOCK A GF COUNTER 108 complete (See Drawing A-045-C108 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 109 - BLOCK A GF COUNTER 109 complete (See Drawing A-045-C109 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 110 - BLOCK A GF COUNTER 110 complete (See Drawing A-045-C110 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 111 - BLOCK A GF COUNTER 111 complete (See Drawing A-045-C111 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 112 - BLOCK A GF COUNTER 112 complete (See Drawing A-045-C112 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 201 - BLOCK A FF COUNTER 201 complete (See Drawing A-045-C201 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 202 - BLOCK A FF COUNTER 202 complete (See Drawing A-045-C202 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 203 - BLOCK A FF COUNTER 203 complete (See Drawing A-045-C203 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 205 - BLOCK A FF COUNTER 205 complete (See Drawing A-045-C205 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 208 - BLOCK A FF COUNTER 208 complete (See Drawing A-045-C208 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 209 - BLOCK A FF COUNTER 209 complete (See Drawing A-045-C209 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 210 - BLOCK A FF COUNTER 210 complete (See Drawing A-045-C210 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 301 - BLOCK A SF COUNTER 301 complete (See Drawing A-045-C301 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 302 - BLOCK A SF COUNTER 302 complete (See Drawing A-045-C302 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 303 - BLOCK A SF COUNTER 303 complete (See Drawing A-045-C303 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 304 - BLOCK A SF COUNTER 304 complete (See Drawing A-045-C304 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 305 - BLOCK A SF COUNTER 305 complete (See Drawing A-045-C305 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 306 - BLOCK A SF COUNTER 306 complete (See Drawing A-045-C306 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 307 - BLOCK A SF COUNTER 307 complete (See Drawing A-045-C307 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 308 - BLOCK A SF COUNTER 308 complete (See Drawing A-045-C308 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 311 - BLOCK A SF COUNTER 311 complete (See Drawing A-045-C311 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D2397*C2397","v":{"v":0,"d":"R0.00"}}]
["Counter 002 - BLOCK B LG COUNTER 002 complete (See Drawing B-045-C002 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 003 - BLOCK B LG COUNTER 003 complete (See Drawing B-045-C003 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 009 - BLOCK B LG COUNTER 009 complete (See Drawing B-045-C009 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 010 - BLOCK B LG COUNTER 010 complete (See Drawing B-045-C010 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 011 - BLOCK B LG COUNTER 011 complete (See Drawing B-045-C011 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 103 - BLOCK B GF COUNTER 103 complete (See Drawing B-045-C103 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 104 - BLOCK C GF COUNTER 104 complete (See Drawing C-045-C104 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 106 - BLOCK C GF COUNTER 106 complete (See Drawing C-045-C106 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 107 - BLOCK C GF COUNTER 107 complete (See Drawing C-045-C107 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 201 - BLOCK C FF COUNTER 201 complete (See Drawing C-045-C201 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 203 - BLOCK C FF COUNTER 203 complete (See Drawing C-045-C203 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 207 - BLOCK C FF COUNTER 207 complete (See Drawing C-045-C207 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 209 - BLOCK C FF COUNTER 209 complete (See Drawing C-045-C209 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 002 - BLOCK D LG COUNTER 002 complete (See Drawing D-045-C002 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 104 - BLOCK D GF COUNTER 104 complete (See Drawing D-045-C104 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 205 - BLOCK D FF COUNTER 205 complete (See Drawing D-045-C205 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 208 - BLOCK D FF COUNTER 208 complete (See Drawing D-045-C208 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 101 - BLOCK F GF COUNTER 101 complete (See Drawing F-045-C101 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 003 - BLOCK A LG COUNTER 003 complete (See Drawing A-045-C003 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 006 - BLOCK A LG COUNTER 006 complete (See Drawing A-045-C006 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 007 - BLOCK A LG COUNTER 007 complete (See Drawing A-045-C007 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 206 - BLOCK A FF COUNTER 206 complete (See Drawing A-045-C206 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 207 - BLOCK A FF COUNTER 207 complete (See Drawing A-045-C207 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 211 - BLOCK A FF COUNTER 211 complete (See Drawing A-045-C211 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 213 - BLOCK A FF COUNTER 213 complete (See Drawing A-045-C213 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 214 - BLOCK A FF COUNTER 214 complete (See Drawing A-045-C214 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 309 - BLOCK A SF COUNTER 309 complete (See Drawing A-045-C309 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 310 - BLOCK A SF COUNTER 310 complete (See Drawing A-045-C310 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 312 - BLOCK A SF COUNTER 312 complete (See Drawing A-045-C312 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 204 - BLOCK D FF COUNTER 204 complete (See Drawing D-045-C204 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 012 - BLOCK B LG COUNTER 012 complete (See Drawing B-045-C012 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 013 - BLOCK B LG COUNTER 013 complete (See Drawing B-045-C013 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D2461*C2461","v":{"v":0,"d":"R0.00"}}]
["Counter 101 - BLOCK B GF COUNTER 101 complete (See Drawing B-045-C101 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 102 - BLOCK B GF COUNTER 102 complete (See Drawing B-045-C102 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 104 - BLOCK B GF COUNTER 104 complete (See Drawing B-045-C104 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 105 - BLOCK B GF COUNTER 105 complete (See Drawing B-045-C105 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 106 - BLOCK B GF COUNTER 106 complete (See Drawing B-045-C106 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 107 - BLOCK B GF COUNTER 107 complete (See Drawing B-045-C107 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 201 - BLOCK B FF COUNTER 201 complete (See Drawing B-045-C201 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 202 - BLOCK B FF COUNTER 202 complete (See Drawing B-045-C202 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 205 - BLOCK B FF COUNTER 205 complete (See Drawing B-045-C205 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 206 - BLOCK B FF COUNTER 206 complete (See Drawing B-045-C206 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 207 - BLOCK B FF COUNTER 207 complete (See Drawing B-045-C207 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 208 - BLOCK B FF COUNTER 208 complete (See Drawing B-045-C208 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 301 - BLOCK B SF COUNTER 301 complete (See Drawing B-045-C301 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 304 - BLOCK B SF COUNTER 304 complete (See Drawing B-045-C304 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 305 - BLOCK B SF COUNTER 305 complete (See Drawing B-045-C305 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 306 - BLOCK B SF COUNTER 306 complete (See Drawing B-045-C306 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 109 - BLOCK C GF COUNTER 109 complete (See Drawing C-045-C109 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 202 - BLOCK C FF COUNTER 202 complete (See Drawing C-045-C202 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 204 - BLOCK C FF COUNTER 204 complete (See Drawing C-045-C204 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 205 - BLOCK C FF COUNTER 205 complete (See Drawing C-045-C205 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 206 - BLOCK C FF COUNTER 206 complete (See Drawing C-045-C206 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 208 - BLOCK C FF COUNTER 208 complete (See Drawing C-045-C208 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 210 - BLOCK C FF COUNTER 210 complete (See Drawing C-045-C210 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 101 - BLOCK D GF COUNTER 101 complete (See Drawing D-045-C101 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 105 - BLOCK D GF COUNTER 105 complete (See Drawing D-045-C105 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 106 - BLOCK D GF COUNTER 106 complete (See Drawing D-045-C106 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 107 - BLOCK D GF COUNTER 107 complete (See Drawing D-045-C107 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 108 - BLOCK D GF COUNTER 108 complete (See Drawing D-045-C108 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 109 - BLOCK D GF COUNTER 109 complete (See Drawing D-045-C109 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 110 - BLOCK D GF COUNTER 110 complete (See Drawing D-045-C110 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 111 - BLOCK D GF COUNTER 111 complete (See Drawing D-045-C111 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 201 - BLOCK D FF COUNTER 201 complete (See Drawing D-045-C201 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D2525*C2525","v":{"v":0,"d":"R0.00"}}]
["Counter 202 - BLOCK D FF COUNTER 202 complete (See Drawing D-045-C202 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 203 - BLOCK D FF COUNTER 203 complete (See Drawing D-045-C203 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 207 - BLOCK D FF COUNTER 207 complete (See Drawing D-045-C207 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 209 - BLOCK D FF COUNTER 209 complete (See Drawing D-045-C209 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 210 - BLOCK D FF COUNTER 210 complete (See Drawing D-045-C210 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 301 - BLOCK D SF COUNTER 301 complete (See Drawing D-045-C301 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 303 - BLOCK D SF COUNTER 303 complete (See Drawing D-045-C303 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 001 - BLOCK D LG COUNTER 001 complete (See Drawing D-045-C001 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 004 - BLOCK A LG COUNTER 004 complete (See Drawing A-045-C004 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 204 - BLOCK A FF COUNTER 204 complete (See Drawing A-045-C204 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 212 - BLOCK A FF COUNTER 212 complete (See Drawing A-045-C212 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 001 - BLOCK B LG COUNTER 001 complete (See Drawing B-045-C001 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 005 - BLOCK B LG COUNTER 005 complete circular on plan (See Drawing B-045-C005 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 301 - BLOCK C SF COUNTER 301 complete (See Drawing C-045-C301 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 006 - BLOCK B LG COUNTER 006 complete (See Drawing B-045-C006 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 007 - BLOCK B LG COUNTER 007 complete (See Drawing B-045-C007 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 008 - BLOCK B LG COUNTER 008 complete (See Drawing B-045-C008 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 014 - BLOCK B LG COUNTER 014 complete (See Drawing B-045-C014 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 015 - BLOCK B LG COUNTER 015 complete (See Drawing B-045-C015 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 102 - BLOCK C GF COUNTER 102 complete (See Drawing C-045-C102 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 004 - BLOCK B LG COUNTER 004 complete circular on plan (See Drawing B-045-C004 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 108 - BLOCK B GF COUNTER 108 complete (See Drawing B-045-C108 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 203 - BLOCK B FF COUNTER 203 complete (See Drawing B-045-C203 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 204 - BLOCK B FF COUNTER 204 complete (See Drawing B-045-C204 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 209 - BLOCK B FF COUNTER 209 complete (See Drawing B-045-C209 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 302 - BLOCK B SF COUNTER 302 complete (See Drawing B-045-C302 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 303 - BLOCK B SF COUNTER 303 complete (See Drawing B-045-C303 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 112 - BLOCK D GF COUNTER 112 complete (See Drawing D-045-C112 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 206 - BLOCK D FF COUNTER 206 complete (See Drawing D-045-C206 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 211 - BLOCK D FF COUNTER 211 complete (See Drawing D-045-C211 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 302 - BLOCK D SF COUNTER 302 complete (See Drawing D-045-C302 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 307 - BLOCK B SF COUNTER 307 complete (See Drawing B-045-C307 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D2589*C2589","v":{"v":0,"d":"R0.00"}}]
["Counter 105 - BLOCK C GF COUNTER 105 complete (See Drawing C-045-C105 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 101 - BLOCK C GF COUNTER 101 complete (See Drawing C-045-C101 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 103 - BLOCK C GF COUNTER 103 complete (See Drawing C-045-C103 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 211 - BLOCK C FF COUNTER 211 complete (See Drawing C-045-C211 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 102 - BLOCK D GF COUNTER 102 complete (See Drawing D-045-C102 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Counter 103 - BLOCK D GF COUNTER 103 complete (See Drawing D-045-C103 attached to the back of these bills of quantities) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PNEUMATIC TUBE SYSTEM - JOINERY AND FITTINGS ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Supply and install Pneumatic Station (PC Amount of R12000.00 per unit, excluding VAT). Rate to include manufacture, transportation, delivery and installation. ","No",59,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TIMBER BENCH, ETC.","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["32mm Meranti slatted seating bench","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["380mm Wide open slatted seat formed of 32 x 70mm x four angle rounded Meranti slats at 100mm centres screwed to 40 x 40 x 3mm thick tubular section rails, with expansion bolts and mitred angle intersections bolted at 1m centres in brickwork of concrete all as per manufactures specification and HDG Fittings and fixtures schedules (CHA042)","m",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["500mm Wide open slatted seat formed of 32 x 70mm x four angle rounded Meranti slats at 100mm centres screwed to 40 x 40 x 3mm thick tubular section rails, with expansion bolts and mitred angle intersections bolted at 1m centres in brickwork of concrete all as per manufactures specification and HDG Fittings and fixtures schedules (CHA042)","m",39,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["700mm Wide open slatted seat formed of 32 x 70mm x four angle rounded Meranti slats at 100mm centres screwed to 40 x 40 x 3mm thick tubular section rails, with expansion bolts and mitred angle intersections bolted at 1m centres in brickwork of concrete all as per manufactures specification and HDG Fittings and fixtures schedules (CHA042)","m",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TOTAL CARPENTRY & JOINERY",{"$nulls":3},{"$f":"SUM(E1903:E2615)","v":{"v":0,"d":"0.00"}}]
[null,null,0,null,{"v":0,"d":"R0.00"}]
["SECTION 2","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NEW HOSPITAL ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["BILL NO 7","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["CEILINGS, PARTITIONS AND ACCESS FLOORING","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PREAMBLES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Preambles for Trades as defined in Scope of Work (C3.1 Item 4.1 & Item 4.2)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TRADE NAMES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Any reference to trade names in the Bills of Quantities or  Architect's specification or drawings shall deem to mean \"or similar and approved\"",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["GENERAL PREAMBLES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Samples - With reference to all items and colour schemes: Samples off all items is to be presented for approval prior to any bulk orders. Please take note that most items will have at least six week delivery period, these approvals will only take place at dates off site meetings, the samples need to be approved well in advance to avoid any delays with lead time on orders. All samples must remain in the sample room for the duration of the contract Mock up rooms – all wall and floor finishes must be prepared in advance as part of a mock up room/rooms and at least a 100 square meter of vinyl flooring will serve as a sample floor.",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SUPPLEMENTARY PREAMBLES","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Descriptions","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Items described as \"nailed\" shall be deemed to be fixed with hardened steel nails or pins or shot pinned to brickwork or concrete",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Items described as \"plugged\" shall be deemed to include screwing to fibre, plastic or metal plugs at not exceeding 600mm centres, and where described as \"bolted\" the bolts have been given elsewhere ____________________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 129 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["INSULATION","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["30mm Thick Isover Hydroboard thermal insulation with compressive strength of 225kPa and thermal conductivity of 0.032W/m.K including all necessary fixing or similar approved. All in accordance with manufacturer's recommendations.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Below surface bed insulation","m2",23335,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D2653*C2653","v":{"v":0,"d":"R0.00"}}]
["75mm Thick Isover Hydroboard thermal insulation with compressive strength of 225kPa and thermal conductivity of 0.032W/m.K including all necessary fixing or similar approved. All in accordance with manufacturer's recommendations.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On concrete slabs to receive screed ","m2",13190,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100mm Thick Isover Aerolite non-combustible light weight fibreglass Glasswool thermal ceiling insulation 12kg/m³ closely fitted with ends butted firmly between tie beams and laid loose on top of brandering between roof timbers or similar approved. All in accordance with manufacturer`s recommendations. (D69)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ceiling insulation","m2",4919,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["METAL CEILING","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Bond-Lok 1mm thick sheet metal ceiling panels with Chromadek finish, installed with concealed screws at max 400 mm c/c to mild steel lip-channel purlins (measured elsewhere) or similar approved. Colours and type to Architect’s approval (D25) ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Steel ceilings ","m2",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["50mm x 50mm x 3mm Angle iron cornice riveted to ceiling","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Galvanised mild steel angle iron cornice","m",9,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NAILED UP CEILINGS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Pelican Systems Jumbo Fibre Cement ceiling system with 6mm thick fibre cement board fixed at right angles to 38 x 38mm battens fixed to concrete at 600mm centres, using 25mm drywall screws at 150mm centres. All joints to be covered with a 6mm JUMBO Jointing Strip and prepared for decoration or similar approved. All in accordance with the manufacturer's instructions. (D3)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ceilings ","m2",6578,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SUSPENDED CEILINGS ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Note:","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Electrical  light  fittings, diffusers, panels, etc generally are \"lay  in\"  units  of  the  same dimensions as the suspension grid described  and  allowance  must  be  made  accordingly  for their support  inclusive  of any flexibility insetting out that may be required (ceiling panels have not been deducted and pricing is to take cognisance thereof)",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Pelican Systems Econocal White vinyl clad calcium silicate aluminium foil backed ceiling tile manufactured in accordance with SANS 428:2012, size 1200 x 600 x 6mm thick, laid on 38 x 24mm pre-painted Exposed Econogrid tee suspension system, comprising of main tees at 1200mm centres and cross tees at 600mm centres. Main tees suspended by means of galvanised strap hangers at 1200mm centres or similar approved. All in accordance with the manufacturer's recommendations. Colour to Architect's approval, complete with SABISA certificate. (D1)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ceilings suspended exceeding 1m and not exceeding 2m on average below concrete soffits","m2",33387,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Pelican Systems Econotherm White vinyl clad calcium silicate aluminium foil backed ceiling tile manufactured in accordance with SANS 428:2012, size 1200 x 600 x 6mm thick, with 55mm glass fibre thermal insulation over ceiling tiles, laid on 38 x 24mm pre-painted Exposed Econogrid tee suspension system, comprising of main tees at 1200mm centres and cross tees at 600mm centres. Main tees suspended by means of galvanised strap hangers at 1200mm centres or similar approved. All in accordance with the manufacturer's recommendations. Colour to Architect's approval, complete with SABISA certificate. (D1)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ceilings suspended not exceeding 1m below concrete soffits","m2",12788,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ceilings suspended exceeding 1m and not exceeding 2m on average below concrete soffits","m2",4989,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ceilings suspended not exceeding 1m below steel purlins (purlins at approximately 1500mm centres, trusses at 5000mm centres) ","m2",8955,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ceilings suspended exceeding 1m and not exceeding 2m on average below steel purlins (purlins at approximately 1500mm centres, trusses at 5000mm centres) ","m2",1274,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ecophon Focus DS 600 x 600 x 20mm thick acoustic white frost square ceiling tiles, installed according to Ecophon installation diagram M206, including all necessary hangers, grids and hold down clips or similar approved. All in accordance with the manufacturer's recommendations and SABISA guidelines. (D105)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ceilings suspended not exceeding 1m below steel purlins (purlins at approximately 1500mm centres, trusses at 5000mm centres) ","m2",239,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Gypceil concealed grid ceiling fire rated ceiling system consisting of 2 layers of gyproc firestop 15mm fixed to a secondary framework of steel brandering. The secondary framework is fixed to the primary framework consisting of donn ultrasteel 51mm suspended using donn galvanised steel angle 25mm x 25mm. 60 minute fire rating.Tested in accordance with SANS 10177:2 or similar approved. All in accordance with the manufacturer's recommendation. Colour to Architect's approval, complete with SABISA certificate. (D44)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ceilings suspended not exceeding 1m below steel purlins (purlins at approximately 1500mm centres, trusses at 5000mm centres) ","m2",92,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ceilings suspended exceeding 1m and not exceeding 2m on average below steel purlins (purlins at approximately 1500mm centres, trusses at 5000mm centres) ","m2",12,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ceilings suspended not exceeding 1m below concrete soffits","m2",22,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ceilings suspended exceeding 1m and not exceeding 2m below concrete soffits","m2",130,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Econo (Code: CGDZ1S36) shadowline wall angle trim or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Shadowline cornice, plugged to walls","m",52631,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but circular on plan ","m",45,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D2717*C2717","v":{"v":0,"d":"R0.00"}}]
["Pelican Systems Jumbo Fibre Cement ceiling system with 4mm thick fibre cement board fixed at right angles to 35mm Jumbo galvanised steel main and cross tees at 400mm centres, using 25mm drywall screws at 150mm centres. All joints to be covered with a 6mm JUMBO Jointing Strip and prepared for decoration or similar approved. All in accordance with the manufacturer's instructions. (D3)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ceilings ","m2",15,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Pelican Systems Jumbo Fibre Cement ceiling system with 6mm thick fibre cement board fixed at right angles to 35mm Jumbo galvanised steel main and cross tees at 400mm centres, using 25mm drywall screws at 150mm centres. All joints to be covered with a 6mm JUMBO Jointing Strip and prepared for decoration or similar approved. All in accordance with the manufacturer's instructions. (D3)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ceilings ","m2",203,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Pelican Systems JUMBO skimmed ceiling system with 9mm thick JUMBO plasterboard fixed at right angles using 25mm Jumbo drywall screws at 150mm centres to JUMBO steel brandering comprising JUMBO steel brandering at 400mm centres in one direction only. All joints to be covered with JUMBO fiba tape and the entire surface plastered with 3mm to 6mm thick JUMBO skimming plaster complete with SABISA certificate (D4) or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ceilings suspended not exceeding 1m below concrete soffits","m2",1491,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ceilings suspended exceeding 1m and not exceeding 2m below concrete soffits","m2",239,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ceilings suspended not exceeding 1m on average below steel purlins (purlins at approximately 1500mm centres, trusses at 5000mm centres) ","m2",138,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ceilings suspended exceeding 1m and not exceeding 2m on average below steel purlins (purlins at approximately 1500mm centres, trusses at 5000mm centres) ","m2",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Pelican Systems JUMBO skimmed ceiling system with 9mm thick JUMBO plasterboard fixed at right angles using 25mm Jumbo drywall screws at 150mm centres to JUMBO steel brandering comprising JUMBO steel brandering at 300mm centres in one direction only. All joints to be covered with JUMBO fiba tape and the entire surface plastered with 3mm to 6mm thick JUMBO skimming plaster complete with SABISA certificate (D15) or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sides of bulkheads, suspending exceeding 1m and not exceeding 2m below concrete","m2",114,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sides of bulkheads, suspending exceeding 2m and not exceeding 3m below concrete","m2",495,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but circular on plan ","m2",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Soffits of  bulkheads, suspending not exceeding 1m below concrete","m2",143,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Soffits of  bulkheads, suspending exceeding 1m and not exceeding 2m below concrete","m2",35,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Soffits of  bulkheads, suspending exceeding 2m and not exceeding 3m below concrete","m2",300,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sides of  bulkheads, suspending not exceeding on average below steel purlins (purlins at approximately 1500mm centres, trusses at 5000mm centres) ","m2",92,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sides of  bulkheads, suspending exceeding 1m and not exceeding 2m on average below steel purlins (purlins at approximately 1500mm centres, trusses at 5000mm centres) ","m2",159,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Soffits of  bulkheads, suspending not exceeding 1m on average below steel purlins (purlins at approximately 1500mm centres, trusses at 5000mm centres) ","m2",59,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Soffits of  bulkheads, suspending exceeding 1m and not exceeding 2m on average below steel purlins (purlins at approximately 1500mm centres, trusses at 5000mm centres) ","m2",112,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Standard metal guard (See Drawings Drawing TYP-044-001 at the back of the Bills of Quantities)","m",1756,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PVC guard circular on plan (See Drawings Drawing TYP-044-001 at the back of the Bills of Quantities)","m",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Pelican Systems JUMBO MR skimmed ceiling system with 12mm thick JUMBO plasterboard fixed at right angles using 25mm Jumbo drywall screws at 150mm centres to JUMBO steel brandering comprising JUMBO steel brandering at 400mm centres in one direction only. All joints to be covered with JUMBO fiba tape and the entire surface plastered with 3mm to 6mm thick JUMBO skimming plaster complete with SABISA certificate (D63) or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ceilings suspended exceeding 1m and not exceeding 2m on average below steel purlins (purlins at approximately 1500mm centres, trusses at 5000mm centres) ","m2",24,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Pelican Systems Aluminium PS4 shadow wall trim, fixed to plastered brickwork with 5 x 25mm wall anchors at 450mm centres or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Shadowline cornice, fixed to walls","m",4497,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Shadowline cornice, fixed to angle ","m",512,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but circular on plan ","m",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Shadowline cornice, fixed to adjacent plasterboard  ","m",1242,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but circular on plan ","m",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["25 x 25  x 2mm Galvanised angle as per detail drawing HDG - TYP-044-006","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Angle fixed to ceiling ","m",512,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D2781*C2781","v":{"v":0,"d":"R0.00"}}]
["Ditto, but circular on plan","m",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ceilings hung in varying height to form artistic ceiling below structural steel, PC amount of Eight Hundred Rand (R 800-00) nett , installed complete at approximately 16m above floor level ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ceilings suspended not exceeding 1m on average below steel purlins (purlins at approximately 1500mm centres, trusses at 5000mm centres) ","m2",1192,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 138 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PARTITIONS ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Unless otherwise described, prices for partitions shall be deemed to include for standard flat section aluminium skirting on both sides",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Drywall 63/30 with overall thickness of 89mm comprising internal framing formed of 63mm galvanised steel studs fixed at 600mm centres to galvanised steel top and bottom track with 63mm thick SoundTherm Insulation of partition, including any additional steel studding necessary at door openings, glazed or other apertures, abutments, ends, corners, etc. and covered with 12mm thick plasterboards in single lengths to suit height, butt jointed and secured to studding with 25mm drywall screws at maximum 220mm centres, the joints taped over and flushed over with jointing compound prepared for painting. (C81) ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Partitioning 2100m high with bottom plugged and top track fixed to suspended ceiling ","m",16,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Partitioning 2400m high with bottom plugged and top track fixed to suspended ceiling ","m",7,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over partition 2400m high for fair end","No",20,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Partitioning 2805m high with bottom plugged and top track fixed to suspended ceiling ","m",2532,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over partition 2805m high for vertical abutment","No",384,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over partition 2805m high for corner","No",79,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over partition 2805m high for obtuse corner","No",24,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over partition 2805m high for T-intersection","No",148,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over partition 2805m high for obtuse-intersection","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over partition 2805m high for fair end including natural anodised 'Drywall' aluminium wall channel","No",45,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Partitioning 2980m high with bottom plugged and top track fixed to suspended ceiling ","m",13,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over partition 2980m high for vertical abutment","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over partition 2980m high for T-intersection","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Firewall 63/30/S46 with overall thickness of 93mm comprising internal framing formed of 63mm galvanised steel studs fixed at 600mm centres to galvanised steel top and bottom track with 63mm thick SoundTherm Insulation of partition, including any additional steel Studding necessary at door openings, glazed or other apertures, abutments, ends, corners, etc. and covered with 15mm thick plasterboards in single lengths to suit height, butt jointed and secured to Stud with 25mm drywall screws at maximum 220mm centres, the joints taped over and flushed over with jointing compound prepared for painting. (C82) ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Partitioning 1300m high with bottom plugged and top track fixed to roof trusses or concrete slab (installed in ceiling void) ","m",657,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over partition 1300m high for vertical abutment","No",68,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Partitioning 1800m high with bottom plugged and top track fixed to roof trusses or concrete slab (installed in ceiling void) ","m",354,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over partition 1800m high for vertical abutment","No",36,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Partitioning 2333m high with bottom plugged and top track fixed to roof trusses or concrete slab","m",34,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over partition 2333m high for vertical abutment","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Partitioning 2550m high with bottom plugged and top track fixed to roof trusses or concrete slab","m",37,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over partition 2550m high for corner","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["High Performance Wall System. Fire 30 min Sound Rw 53 dB Skimmed consisting of 1 layer 12.5mm, (non-combustible) fixed to both sides of the framework using board Sharp Point Screws 3.5mm diameter x 25mm at maximum 220mm centres. 102mm x 35mm Studs (0.4mm thickness, Rigidised, indexed service holes, Z150 galvanise coating, locally manufactured, recycled content, ISO 9001 & 14001 certification) friction fitted into top and bottom of track 102mm x 25mm at 600mm centres. Floor and head Track fixed with two lines of staggered fixings 50mm apart and spaced at 600mm centres. Track 102mm x 50mm shall be used in areas subject to deflection. Install 102mm (locally manufactured, recycled content, ISO 9001 & 14001 certification) into the cavity with joints tightly butted, leaving no gaps. Apply Tape to all joints and internal corners. Install Corner Bead to all external corners. Cover Tape with one layer of Jointing plaster. Skim the surface using one layer of Skimming plaster. (C79)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Partitioning 4420mm high with bottom track plugged and top track fixed to soffit of concrete slab","m",80,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over partition 4420mm high for vertical abutment","No",16,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D2845*C2845","v":{"v":0,"d":"R0.00"}}]
["ALUMINIUM, GLAZED AND DRYWALL PARTITION","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Aluminium, glazed and drywall partition with solid aluminium panel 900mm high, glazed screen above to 2125mm high fixed to and including 75 x 75 x 2.5 SHS beam at 2125mm above finished floor level suspended from slab above, and 680mm high Gyproc Classic Wall System 63/F30S42 Ultrasteel Stud Drywall to underside of ceiling with fire rating of 30 minutes (SANS 10177-2) and sound rating of 42dB, consisting of 1 layer Gyproc RhinoBoard 12.5mm fixed to both sides of the framework, stud and track system with 63,5 x 35mm Donn Drywall UltraSTEEL™ studs at recommended centres, friction fitted into head track and SHS steel member, clad on both sides with all external angles to have drywall corner beads attached and all joints to be covered with RhinoTape and finished with one layer of RhinoLite applied and lightly sanded down, leaving wall surface prepared for painting or similar approved. All in accordance with the manufacturer`s recommendations","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Partitioning 2805mm high overall","m",185,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over partition 2805mm high for vertical abutment","No",66,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over partition 2805mm high for corner","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over partition 2805mm high for obtuse corner","No",10,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over partition 2805mm high for T-intersection","No",13,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over partition 2805mm high for fair end including natural anodised drywall aluminium wall channel","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["EXTERNAL MAGNESIUM OXIDE BOARDS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["12mm thick Supertec Magnesium Oxide boards wall cladding bud jointed, size 1200 x 300, installed to existing plastered wall with 40mm plugged and countersink stainless steel screws at max 50mm c/c in both directions (max 75mm from edge) and ensure all board edges is flush with adjoining boards. Refer to detail drawings and colours to Architects approval with a pre-approved sample installation. Finish with Versus Texture finishes(H14) elsewhere. (Suptertec 011 8684900) or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Magnesium Oxide Boards 3.4m high fixed to brickwork or concrete","m",44,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over Magnesium Oxide Boards 3.4m high for corner","No",8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Magnesium Oxide Boards 4.12m high fixed to brickwork or concrete","m",80,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over Magnesium Oxide Boards 4.12m high for corner","No",16,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["DOORS, SIDELIGHTS AND WINDOWS IN PARTITIONING","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Doors","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra  over partition for polyester powder coated aluminium  door  frame for 40mm door with  one  pair  of  100mm nylon washered aluminium  hinges  including additional studding, trimming, etc (door and ironmongery elsewhere)","H4",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Door size 813 x 1738mm","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Door size 813 x 2032mm","No",62,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Door size 813 x 2032mm with 279mm high fanlight above","No",16,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Door size 965 x 2032mm ","No",13,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Door size 1264 x 2032mm ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Double door size 1350 x 2032mm with  two  pairs  of  100mm nylon washered aluminium  hinges ","No",7,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Double door size 1588 x 2032mm with  two  pairs  of  100mm nylon washered aluminium  hinges ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Double door size 1800 x 2032mm with  two  pairs  of  100mm nylon washered aluminium  hinges","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["AUDIO BOOTH INSTALLATION ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Provide the sum of R100 000.00 (One Hundred Thousand Rand) nett for Audio Booth Installation","Item",1,{"v":100000,"d":"R100,000.00"},{"v":100000,"d":"R100,000.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for profit if required ","%IT",1,null,{"$f":"D2900*C2900","v":{"v":0,"d":"R0.00"}}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for attendance","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["ACCESS FLOORING ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Lafarge Gypsum (011-389 4500) Snap-on Stringer access floor system with 600 x 600mm Type 2 steel clad cementitious core panels with factory bonded conductive and anti-static vinyl finish, supported by and including all necessary understructure components as per the manufacturer's specification for a finished floor height of not exceeding 595mm high above concrete sub-floor (elsewhere measured) all in accordance with SANS 1549:1992. Colour to Architects approval.  System to include decorative border  integral trim finish, access grommets, air diffusers, perforated panels, electric power boxes, additional bracing, 1mm galvanised mild steel fire barrier and all holes and sealing (A13) or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Access floor system ","m2",102,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D2909*C2909","v":{"v":0,"d":"R0.00"}}]
["CEILINGS, PARTITIONS AND ACCESS FLOORING",{"$nulls":3},{"$f":"SUM(E2617:E2909)","v":{"v":100000,"d":"100,000.00"}}]
[null,null,0,null,{"v":0,"d":"R0.00"}]
["SECTION 2","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NEW HOSPITAL ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["BILL NO 8","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["FLOOR COVERINGS, WALL LININGS, ETC","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PREAMBLES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Preambles for Trades as defined in Scope of Work (C3.1 Item 4.1 & Item 4.2)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TRADE NAMES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Any reference to trade names in the Bills of Quantities or  Architect's specification or drawings shall deem to mean \"or similar and approved\"",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["GENERAL PREAMBLES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Samples - With reference to all items and colour schemes: Samples off all items is to be presented for approval prior to any bulk orders. Please take note that most items will have at least six week delivery period, these approvals will only take place at dates off site meetings, the samples need to be approved well in advance to avoid any delays with lead time on orders. All samples must remain in the sample room for the duration of the contract. Mock up rooms – all wall and floor finishes must be prepared in advance as part of a mock up room/rooms and at least a 100 square meter of vinyl flooring will serve as a sample floor.",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 130 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["FLOOR COVERINGS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Polyflor 2mm thick Paletone PUR Homogeneous vinyl floor sheeting (colour to architects approval), laid in acrylic adhesive spread with a notched trowel on suitably prepared cement screed floors with a hygrometer reading showing a moisture content of less than 70%, with joints welded with a fully flexible coloured Polyflor welding rod to provide a smooth, hygienic sealed finish and rolled with 68kg articulated floor roller or similar approved. All in accordance with manufacturer`s recommendations. (A47)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Seamless vinyl floor sheets on floors","m2",47926,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over for waving patterns in different colours including all necessary cutting and welding (Allow for 30% waste factor) ","m2",2758,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["200mm Wide border x  200mm high turn up against walls (400mm girth), including welding to floor covering (floor covering elsewhere) including all formed internal and external corners","m",36114,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but circular on plan ","m",24,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Polyflor 2mm thick slip resistant Polysafe Verona PUR Safety vinyl floor sheeting (colour to architects approval), laid in acrylic adhesive spread with a notched trowel on suitably prepared cement screed floors, with a hygrometer reading showing a moisture content of less than 70%, with joints welded with a fully flexible coloured Polyflor welding rod to provide a smooth, hygienic sealed finish and rolled with 68kg articulated floor roller or similar approved. All in accordance with manufacturer`s recommendations. (A2)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Seamless vinyl floor sheets on floors","m2",3582,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["200mm Wide border x  200mm high turn up against walls (400mm girth), including welding to floor covering (floor covering elsewhere) including all formed internal and external corners","m",6382,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but circular on plan ","m",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Polyflor 2mm thick slip resistant Polysafe Hydro Evolve Safety vinyl floor sheeting (colour to architects approval), laid in acrylic adhesive spread with a notched trowel on suitably prepared cement screed floors, with a hygrometer reading showing a moisture content of less than 70%, with joints welded with a fully flexible coloured Polyflor welding rod to provide a smooth, hygienic sealed finish and rolled with 68kg articulated floor roller or similar approved. All in accordance with manufacturer`s recommendations. (A12)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Seamless vinyl floor sheets on floors","m2",656,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["200mm Wide border x  200mm high turn up against walls (400mm girth), including welding to floor covering (floor covering elsewhere) including all formed internal and external corners","m",1479,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Polyflor 2mm thick OHMega EC ESD vinyl floor sheeting (colour to architects approval), laid in conductive acrylic adhesive spread with a notched trowel on suitably prepared cement screed with a hygrometer reading showing a moisture content of less than 70%, with joints welded with a fully flexible coloured Polyflor welding rod to provide a smooth, hygienic sealed finish and rolled with 68kg articulated floor roller or similar approved. All in accordance with manufacturer`s recommendations. (A18)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Seamless vinyl floor sheets on floors","m2",1740,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["200mm Wide border x  200mm high turn up against walls (400mm girth), including welding to floor covering (floor covering elsewhere) including all formed internal and external corners","m",1058,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Polyflor 3.7mm thick Silentflor PUR Heterogeneous vinyl floor sheeting with a 0.65mm clear wear layer (colour to architects approval), laid in an approved adhesive spread with a notched trowel on suitably prepared cement screed with a hygrometer reading showing a moisture content of less than 70%, with joints welded with a fully flexible coloured Polyflor welding rod to provide a smooth, hygienic sealed finish and rolled with 68kg articulated floor roller or similar approved. All in accordance with manufacturer's recommendations. (A138)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Seamless vinyl floor sheets on floors","m2",926,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sundries","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Circular cutting to vinyl sheeting","m",34,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D2973*C2973","v":{"v":0,"d":"R0.00"}}]
["WALL LININGS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Polyflor 2.5mm thick smooth Sure Protect Pure PVC-U wall cladding (colour to architects approval), including all trimming, silicone joint sealing, adhesive solutions etc. or similar approved. All in accordance with manufacturer`s recommendations (C42)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On walls","m2",1289,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On partitions","m2",126,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SKIRTINGS, NOSINGS, ETC","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cappings, cove formers, etc ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Polyflor Polycove cove former PC20 colour Black, size 20 x 20mm wide or similar approved. All in accordance with manufacturer`s specifications.","m",45032,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but circular on plan ","m",25,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Polyflor Clip-Top base CB30, size 29.5 x 5.4mm high, glue to wall with an approved adhesive or similar approved. All in accordance with manufacturer`s specifications.","m",37170,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but circular on plan ","m",25,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Polyflor Clip-Top capping CTC30 or similar approved. All in accordance with manufacturer`s specifications.","m",37170,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but circular on plan ","m",25,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Polyflor Polycap vinyl capping strip CS48 colour to architects approval, size 40mm high or similar approved. All in accordance with manufacturer`s specifications.","m",6383,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Polyflor Polycap tile capping strip TC48 colour to architects approval, size 40mm high or similar approved. All in accordance with manufacturer`s specifications.","m",1479,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over for Polyflor Polycove taper end piece PC20 colour Black, size 150 x 20mm long or similar approved. All in accordance with manufacturer`s specifications. ","No",10974,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["MOISTURE BARRIER ON FLOORS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ensure surfaces are free of paint, greases, oils and other contaminants and the pores of the base floor are open and suitably prepared to receive the moisture barrier. Apply an extremely high density, moisture tolerant, chemically enhanced 100% solids epoxy moisture barrier coat that prevents the passage of water vapour and moisture through concrete slabs to be applied as per the manufacturer's instruction in at least 2 coats at 90 degrees to each other","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Approved moisture barrier on new screed","m2",6292,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["CARPETS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Medium commercial (SABS use class U4), 100% Polypropylene, 7mm thick needlepunch 3.66m wide broadloom carpet with SABS Class 2 fire rating, weighing 950g/m2, with non-woven primary backing and POWERbac woven synthetic secondary backing, treated with Stain Shield Fibre soil resistant treatment.  Laid on 1200g/m2 underfelt in accordance with SANS 1419:1997, all installed by an approved installer in accordance with SANS 10186:2000.  All install strictly to manufacturer’s specifications on well-prepared screed. Colour and type to Architect’s approval. (A5). Provide the PC amount of R300.00/m² supplied and delivered to site","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Stretch carpet sheets on floors","m2",2965,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Heavy commercial (SABS use class U5) Xentrys Heatset Nylon 6, tufted, with SABS Class 2 fire rating, fibre weight of 1110g/mAC and total weight of 2020mAC, with Powerbac backing. Manufactured in accordance with SANS 1375:2005 laid on 6.5mm thick Eco-Lay (PC Amount of R400.00/m2) supplied and installed)  all installed by an approved installer in accordance with SANS 10186:2000.  All install strictly to manufacturer’s specifications on well-prepared screed. Colour and type to Architect’s approval. (A7) Provide the PC amount of R450.00/m² supplied and delivered to site","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Stretch carpet sheets on floors","m2",102,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Stretch carpet sheets on treads and risers of stepped floors","m2",245,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Stretch carpet sheets on treads and risers of stairs","m2",9,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Circular cutting","m",141,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["12mm Genesis TrakMat (Code EM8902) loop pile entrance mats - light to medium traffic in aluminium sections linked by semi-rigid pvc. Mats to be in recessed floor, complete matwell frame 6113 with Genesis corner angles 161104 and feet 161103, bedded into screed or similar approved. All in accordance with the manufacturer's recommendations","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Matt size 1000 x 1700mm (DST001)","No",29,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Matt size 1000 x 2500mm (DST001)","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Matt size 1500 x 2500mm (DST001)","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Matt size 2500 x 5500mm (DST001)","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["BUMPER RAILS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D3037*C3037","v":{"v":0,"d":"R0.00"}}]
["Wall Guard complete with end caps including reveal and fixings, 50mm aluminium fixing clips, internal PVCu bumper and PVC-u cover. All installed strictly to manufacturers specifications. (BUM019)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["High impact PVC wall guard fixed to wall","m",13957,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over for stop ends, etc.","No",10080,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Heavy duty black rubber wall guard. Installed to wall with approved adhesive strictly to manufacturers specifications. (BUM023)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Wall guard fixed to wall","m",148,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over for stop ends, etc.","No",46,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["WALL AND CORNER PROTECTORS, ETC.","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["75 x 75mm High Impact corner guard (90 degree) with bacterial /fungal growth resistant PVC-u. Installed from skirting level to 700/775mm above FF Level (length to suit skirting level). Installed strictly to manufacturers specifications. (BUM034)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Corner guard","No",1132,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["75 x 75mm High Impact corner guard (90 degree) with bacterial /fungal growth resistant PVC-u. Installed from skirting level to 900mm above FF Level (length to suit skirting level). Installed strictly to manufacturers specifications. (BUM033)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Corner guard","No",50,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100 x 100mm heavy duty black rubber corner guard. Installed to wall with approved adhesive strictly to manufacturers specifications. (BUM024)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Corner guard","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["60 x 60mm Flexi-angle corner guard (90 degree with tape) with bacterial /fungal growth resistant PVC-u. Installed from skirting level to 700/775mm above FF Level (length to suit skirting level). Installed strictly to manufacturers specifications. (BUM016)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Corner guard","No",88,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Standard 150 x 3,5mm wall strip (with tape) with scratch and stain resistant PVC-u. Installed from skirting level to 900mm above FF Level. Installed strictly to manufacturers specifications BUM040","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Wall strip tape","m",2983,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["EXPANSION JOINTS COVERS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Vexcolt Maxatec expansion joint profile (Code: V100-A01-075-35) or similar approved. All in accordance with manufacturer`s specifications","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Expansion joint in floor ","m",1500,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TOTAL FLOOR COVERINGS, WALL LININGS, ETC",{"$nulls":3},{"$f":"SUM(E2911:E3077)","v":{"v":0,"d":"0.00"}}]
[null,null,0,null,{"v":0,"d":"R0.00"}]
["SECTION 2","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NEW HOSPITAL ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["BILL NO 9","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["IRONMONGERY ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PREAMBLES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Preambles for Trades as defined in Scope of Work (C3.1 Item 4.1 & Item 4.2)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TRADE NAMES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Any reference to trade names in the Bills of Quantities or  Architect's specification or drawings shall deem to mean \"or similar and approved\"",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 132 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["IRONMONGERY TO TIMBER DOORS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["HINGES, BOLTS, ETC.","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D3101*C3101","v":{"v":0,"d":"R0.00"}}]
["Assa Abloy or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Union 102 x 76mm ball bearing butt hinge (Code: IW3001SS)","Pairs",3655,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Union Grade 304 stainless steel rising butt hinge (Code: QS4440 LH)","Pairs",302,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Union flush pull handle (Code: IW1492SS)","No",49,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["200 x 19mm Nickel plated lever flush bolt (Code: IW4123SS) fixed with matching screws.","No",752,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["CATCHES, CABIN HOOKS, ETC.","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Assa Abloy or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Stainless steel adjustable roller catch (Code: IW5054SS)","No",924,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Floor mounted door holder (Code: 401SC)","No",630,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["LOCKS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Assa Abloy or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Union 79 x 96mm mortice deadlock (Code: IW2219SS)","No",76,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Union 108 x 78mm Commercial grade Euro style deadlock (Code: IW2219SS)","No",692,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Union 108 x 78mm Commercial grade Euro style latch lock with drawback and silent latch feature (Code: IW2207SS)","No",301,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Union 129 x 78mm Commercial grade emergency exit latch lock (Code: L-2349-78SS)","No",522,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Union oval profile mortice sliding door lock (Code: IW2038SS)","No",12,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Union oval 32mm half knob cylinder (Code: IW2074NP)","No",12,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Rebate conversion set (Code: IW2140SS) ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["32mm Commercial use grand master keyed half cylinder (Code: IWI2081NPMK)","No",24,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["65mm Commercial use grand master keyed double cylinder (Code: IWI2051NPMK)","No",1045,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["65mm Commercial use grand master keyed double turn knob cylinder (Code: IW2061NPMK)","No",340,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Union 8mm WC deadlock (Code: IW2031)","No",808,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Euro style stainless steel cylinder escutcheon (Code: IW1906CYLSS)","No",2542,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Union profile escutcheon (Code: IW1906CYLSS)","No",12,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["HANDLES","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Assa Abloy or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Union Dove pull handle on 192 x 45mm back plate (Code: IW1320/170/4.5*19.2)","Pairs",460,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Union Sandpiper 32mm diameter x 350mm girth stainless steel back to back pull handle (Code: IW1320/325X2/IWFSBTB25)","Pairs",202.5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Union Sandpiper 22mm diameter x 225mm girth stainless steel bolt-through pull handle (Code: IW1320/325)","No",524,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Union Sandpiper 32mm diameter x 350mm girth stainless steel bolt through pull handle (Code: IW1320/325)","No",321,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Union Dove lever handle on 178 x 152mm backplate (Code: IW1051/SBP4CYLSS)","No",301,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Union Dove lever handle and WC indicator on 178 x 152mm backplate (Code: IW1320/170/PPH.17*.15/1921)","No",1616,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D3165*C3165","v":{"v":0,"d":"R0.00"}}]
["Stainless steel pull handle 25mm diameter x 250mm girth with backplate size 94 x 315 x 1.6mm (Code: IW1320/325/PPH9.4*31.5)","No",2538,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["94 x 315mm Stainless steel back plate (Code: PPH1.2*9.4*31.5)","No",524,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PUSH PLATES AND KICKING PLATES","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["1,2mm Thick Grade 304 non-magnetic stainless steel door cladding fixed to timber door with 2.9 x 13mm stainless steel countersunk self tapping screws and \"Genkem Van 497\" adhesive (304SS)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Push plate 200mm high for 450mm wide door ","No",486,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Push plate 200mm high for 493mm wide door ","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Push plate 200mm high for 505mm wide door ","No",46,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Push plate 200mm high for 600mm wide door","No",8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Push plate 200mm high for 686mm wide door","No",38,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Push plate 200mm high for 718mm wide door","No",400,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Push plate 200mm high for 755mm wide door","No",16,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Push plate 200mm high for 762mm wide door","No",54,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Push plate 200mm high for 794mm wide door","No",304,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Push plate 200mm high for 813mm wide door","No",232,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Push plate 200mm high for 868mm wide door","No",960,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Push plate 200mm high for 900mm wide door","No",1142,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Push plate 200mm high for 957mm wide door","No",30,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Push plate 200mm high for 965mm wide door","No",1128,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Push plate 200mm high for 1000mm wide door","No",156,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Push plate 200mm high for 1036mm wide door","No",92,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Push plate 200mm high for 1200mm wide door","No",22,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Push plate 200mm high for 1350mm wide door","No",14,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Push plate 200mm high for 1352mm wide door","No",12,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Push plate 200mm high for 1565mm wide door","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Push plate 200mm high for 1952mm wide door","No",8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Kick plate 200mm high for 450mm wide door","No",392,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Kick plate 200mm high for 493mm wide door","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Kick plate 200mm high for 505mm wide door","No",46,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Kick plate 200mm high for 600mm wide door","No",8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Kick plate 200mm high for 686mm wide door","No",38,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Kick plate 200mm high for 718mm wide door","No",400,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Kick plate 200mm high for 755mm wide door","No",16,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D3229*C3229","v":{"v":0,"d":"R0.00"}}]
["Kick plate 200mm high for 762mm wide door","No",54,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Kick plate 200mm high for 794mm wide door","No",304,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Kick plate 200mm high for 813mm wide door","No",256,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Kick plate 200mm high for 868mm wide door","No",960,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Kick plate 200mm high for 900mm wide door","No",1048,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Kick plate 200mm high for 957mm wide door","No",30,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Kick plate 200mm high for 965mm wide door","No",1150,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Kick plate 200mm high for 1000mm wide door","No",156,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Kick plate 200mm high for 1036mm wide door","No",92,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Kick plate 200mm high for 1200mm wide door","No",22,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Kick plate 200mm high for 1350mm wide door","No",14,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Kick plate 200mm high for 1352mm wide door","No",12,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Kick plate 200mm high for 1565mm wide door","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Kick plate 200mm high for 1952mm wide door","No",8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Bumper plate 1000mm high for 813mm wide door","No",482,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Bumper plate 1000mm high for 965mm wide door","No",1572,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Bumper plate 1000mm high for 1000mm wide door","No",166,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["DOOR PROTECTION","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["National Dairy Equipment (031 700 5444) Grade 304 non magnetic stainless steel door protection or similar approved. Fixed in accordance with the manufacturer's instructions ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Standard edge channel 20 x 40 x 1000mm long","No",1713,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Hinge channel 20 x 40 x 1000mm long channel with cut-out for 100 x 75mm butt hinge","No",3237,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Rebate protection angle 19 x 19 x 1000mm long","No",3048,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["DOOR CLOSERS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Assa Abloy or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cam motion door closer (Code: QS700/QS7703 EN2-3)","No",170,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cam motion door closer (Code: QS750/1/QS7703 EN2-5)","No",1105,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cam motion door closer with delayed action (Code: QS700DA/QS7703 EN2-3)","No",321,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cam motion door closer with integrated mechanical coordinator (Code: QS750X2/QS761)","No",259,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cam motion door closer with integrated electro mechanical hold open device (Code: QS760/ET - SINGLE DOOR)","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Union transom closer 2-5 hold open (Code: QS900HO)","No",55,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Union stainless steel door brace for 774 transom closer (Code: SS-DB774)","No",55,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Union rack & pinion closer 3-5 hold open (Code: QS750/QS7706)","No",40,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D3293*C3293","v":{"v":0,"d":"R0.00"}}]
["Dorma floor pivot bearing (Code: QS5501 pivot 250kg)","No",55,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Dorma double action bottom strap (Code: QS8815 door strap ADJ)","No",55,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SLIDING DOOR TRACKS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Henderson or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Henderson Pacer straight sliding system, comprising 600 aluminium top track, face fixed to wall with 1B brackets, 57B hangers, 94X guide channel, 106N/94 bottom guides with 601P clip stops to suit opening 1500mm wide","Sets",35,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Henderson Pacer straight sliding system, comprising 600 aluminium top track, face fixed to wall with 1B brackets, 57B hangers, 94X guide channel, 106N/94 bottom guides with 601P clip stops to suit opening 1800mm wide","Sets",12,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Besam Unislide automatic bi-parting sliding door mechanism with electronic control unit with plugs in modules, radars, micro cells, electric lock, battery, Exu-PCB, 5-position control switch (off - exit - auto width - open), interlocking between two operators, epoxy colour coated pelmet, colour to Architect's approval, to suit 2000mm opening (SL500)","Sets",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SUNDRIES","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Assa Abloy or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Stainless steel floor mounted door stop (Code: IW5002SC) ","No",123,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Union 27mm wall door stop (Code: IW5005H)","No",4676,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Union 82mm wall projection door stop (Code: IW5005SS)","No",4676,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["IRONMONGERY TO ALUMINIUM DOORS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["HINGES, BOLTS, ETC.","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Assa Abloy or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Union 100 x 75mm ball bearing sinkless hinge (Code: IW3042SS)","Pairs",518,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["HBS aluminium systems HEX 100 standard hinge","Pairs",190,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Flush bolt 180 x 20mm anodised aluminium (Code: M460)","No",84,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["CATCHES, CABIN HOOKS, ETC.","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Assa Abloy or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Stainless steel adjustable roller catch (Code: IW5054SS)","No",429,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["LOCKS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Assa Abloy or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Union 35mm swing bolt (Code: IW2013SS)","No",93,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Union 35mm dead lock (Code: IW2013SS)","No",292,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Union 35mm dead lock/roller catch (Code: IW2024SS)","No",141,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Union narrow stile hook bolt lock Euro profile 174 x 38mm commercial grade (Code: IW2038SS)","No",84,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Union 180mm flush bolt for aluminium doors (Code: M460)","No",114,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["32mm Commercial use grand master keyed half cylinder (Code: IWI2081NPMK)","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["65mm Commercial use grand master keyed double cylinder (Code: IW2061NPMK)","No",608,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Stainless steel narrow stile escutcheon (Code: IW1903CYLSS)","No",1042,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Stainless steel narrow stile escutcheon (Code: IW1903CYLSS)","No",312,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D3357*C3357","v":{"v":0,"d":"R0.00"}}]
["HANDLES","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Assa Abloy or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Union back to back cranked pull handle (Code: QS2301 CRANKED D)","Pairs",138,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Union back to back D-shaped pull handle (Code: IW1320/325X2/IWFSBTB25)","Pairs",157,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Union Sandpiper 22mm diameter x 150mm girth stainless steel bolt-through pull handle (Code: IW1320/170)","No",11,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Union flush pull handle (Code: IW1492SS)","No",198,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["DOOR CLOSERS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Assa Abloy or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Union transom closer 2-5 hold open (Code: QS900HO)","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Dorma floor pivot bearing (Code: QS5501 pivot 250kg)","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Dorma double action bottom strap (Code: QS8815 door strap ADJ)","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SLIDING DOOR TRACKS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Besam or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Besam SL500-2 Unislide sliding door mechanism","Sets",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Besam automatic bi-parting sliding door operator to suit 2000mm opening","Sets",20,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SUNDRIES","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Assa Abloy or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Union 27mm wall door stop (Code: IW5005H)","No",1214,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Union 82mm wall projection door stop (Code: IW5005SS)","No",1198,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Patent screws and nuts (Code: QS4493)","No",7839,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Patent screws and nuts (Code: IWFSM4)","No",2766,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["IRONMONGERY TO GATES","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["LOCKS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Assa Abloy or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["65mm Commercial use grand master keyed double cylinder (Code: IWI2051NPMK)","No",8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Union Euro profile commercial grade mortice hook lock with latch 25mm set back (Code: QH25X85MM-SS)","No",8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["HANDLES","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Assa Abloy or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Union Dove 150mm back to back pull handle (Code: IW1320/170X2/IWFSBTB19 and iw1320/170 and iwfsbtb19)","Pairs",8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SUNDRIES","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Assa Abloy or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Union 27mm wall door stop (Code: IW5005H)","No",72,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D3421*C3421","v":{"v":0,"d":"R0.00"}}]
["Union 82mm wall projection door stop (Code: IW5005SS)","No",72,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["IRONMONGERY TO STEEL DOORS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["HINGES, BOLTS, ETC.","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Assa Abloy or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Union 102 x 76mm ball bearing butt hinge (Code: IW3001SS)","Pairs",152,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["200mm Heavy duty necked barrel bolt (Code: EB5018)","No",76,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["CATCHES, CABIN HOOKS, ETC.","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["LOCKS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["HANDLES","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Assa Abloy or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Union Sandpiper 22mm diameter x 150mm girth stainless steel bolt-through pull handle (Code: IW1320/170)","No",76,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["DOOR CLOSERS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Assa Abloy or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cam motion door closer (Code: QS750/1/QS7703 EN2-5)","No",76,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SUNDRIES","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Assa Abloy or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Union 27mm wall door stop (Code: IW5005H)","No",152,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Union 82mm wall projection door stop (Code: IW5005SS)","No",152,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["BLINDS   ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Manually operated 50mm standard privacy and light control aluminium venetian blinds including De Luxe 50x50mm headrail  with brass cord lock and galvanised tilt mechanism fixed to one side of headrail, including heavy duty universal box brackets complete with matching authentic wood bottom rail, valance, bottom buttons and tassels. Size of blinds to be measured to fit within the window reveal and fixed to underside of lintel. Installed strictly to manufacturer's specification and colour and sample to be pre-approved by Architect (LVR001)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 290 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 325 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 450 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 520 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 540 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 547 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 555 x 1200mm wide","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 555 x 1500mm wide","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 600 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 600 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 640 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 660 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D3485*C3485","v":{"v":0,"d":"R0.00"}}]
["Blind to suit window size 675 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 685 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 690 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 700 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 700 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 704 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 740 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 750 x 1800mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 765 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 790 x 2100mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 790 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 800 x 1200mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 803 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 810 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 820 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 830 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 840 x 1800mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 865 x 900mm wide","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 870 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 900 x 870mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 900 x 900mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 900 x 1200mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 900 x 1500mm high","No",32,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 900 x 1800mm high","No",17,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 900 x 2400mm high","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 925 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 962 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 967 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 970 x 1500mm high","No",8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 985 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 989 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1000 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D3549*C3549","v":{"v":0,"d":"R0.00"}}]
["Blind to suit window size 1014 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1020 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1020 x 1800mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1030 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1050 x 1800mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1065 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1095 x 1200mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1100 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1105 x 1200mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1105 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1120 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1140 x 900mm high","m",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1170 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1180 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1190 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1196 x 1500mm wide","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1200 x 1200mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1200 x 1500mm high","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1230 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1240 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1260 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1260 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1265 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1280 x 1500mm high","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1300 x 1800mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1300 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1305 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1305 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1310 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1320 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1340 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1350 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D3613*C3613","v":{"v":0,"d":"R0.00"}}]
["Blind to suit window size 1355 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1370 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1385 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1400 x 1500mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1400 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1405 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1410 x 1800mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1415 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1425 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1430 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1430 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1440 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1445 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1450 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1490 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1500 x 1500mm high","No",13,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1500 x 1800mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1520 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1520 x 1800mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1525 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1530 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1540 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1550 x 2400mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1555 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1580 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1585 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1595 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1595 x 2100mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1597 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1600 x 2100mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1600 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1610 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D3677*C3677","v":{"v":0,"d":"R0.00"}}]
["Blind to suit window size 1610 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1650 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1660 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1660 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1670 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1675 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1698 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1700 x 1200mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1710 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1705 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1735 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1740 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1740 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1745 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1751 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1755 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1760 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1760 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1765 x 1200mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1770 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1780 x 1500mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1790 x 1800mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1795 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1800 x 900mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1800 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1800 x 1500mm high","No",37,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1800 x 1800mm high","No",24,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1800 x 2100mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1800 x 2400mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1815 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1825 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1829 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D3741*C3741","v":{"v":0,"d":"R0.00"}}]
["Blind to suit window size 1860 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1863 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1870 x 1500mm high","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1875 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1880 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1895 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1900 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1906 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1910 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1925 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1940 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1953 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1970 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1980 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1980 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1980 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1985 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1990 x 1800mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 1995 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2000 x 1500mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2000 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2013 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2025 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2035 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2055 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2065 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2075 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2081 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2090 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2095 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2100 x 1500mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2125 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D3805*C3805","v":{"v":0,"d":"R0.00"}}]
["Blind to suit window size 2145 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2155 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2190 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2100 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2100 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2155 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2157 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2160 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2165 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2190 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2200 x 1800mm high","No",20,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2200 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2205 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2215 x 1200mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2220 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2225 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2226 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2227 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2257 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2260 x 1200mm high","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2260 x 1500mm high","No",12,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2260 x 1800mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2260 x 2400mm high","No",8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2269 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2280 x 1800mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2290 x 1500mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2300 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2305 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2310 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2348 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2360 x 1500mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2370 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D3869*C3869","v":{"v":0,"d":"R0.00"}}]
["Blind to suit window size 2370 x 1800mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2370 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2377 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2395 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2400 x 900mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2400 x 1500mm high","No",13,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2400 x 1800mm high","No",13,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2400 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2405 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2410 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2412 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2420 x 1200mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2430 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2430 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2445 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2470 x 1800mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2487 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2500 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2500 x 1800mm high","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2500 x 2400mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2505 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2505 x 2400mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2510 x 2100mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2515 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2525 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2530 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2530 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2535 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2545 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2555 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2570 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2580 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D3933*C3933","v":{"v":0,"d":"R0.00"}}]
["Blind to suit window size 2590 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2595 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2610 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2620 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2620 x 2400mm high","No",8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2630 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2640 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2640 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2650 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2670 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2670 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2689 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2690 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2700 x 900mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2700 x 1500mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2700 x 1800mm high","No",20,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2700 x 2100mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2700 x 2400mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2705 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2720 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2725 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2725 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2730 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2735 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2750 x 1500mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2750 x 1800mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2770 x 1500mm wide","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2765 x 1200mm wide","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2775 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2790 x 1500mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2795 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2800 x 1800mm high","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D3997*C3997","v":{"v":0,"d":"R0.00"}}]
["Blind to suit window size 2805 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2810 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2820 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2825 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2830 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2840 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2860 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2870 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2835 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2845 x 1500mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2855 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2865 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2875 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2885 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2890 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2895 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2900 x 1800mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2906 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2910 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2910 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2915 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2920 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2925 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2937 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2948 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2965 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2970 x 1500mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2970 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2980 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 2990 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3000 x 1500mm high","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3000 x 2100mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D4061*C4061","v":{"v":0,"d":"R0.00"}}]
["Blind to suit window size 3000 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3010 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3015 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3040 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3040 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3040 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3045 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3055 x 1200mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3055 x 1500mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3060 x 1500mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3067 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3085 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3090 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3093 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3095 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3110 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3125 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3135 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3170 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3190 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3200 x 2400mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3205 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3206 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3220 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3235 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3240 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3245 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3260 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3265 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3285 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3270 x 1200mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3293 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D4125*C4125","v":{"v":0,"d":"R0.00"}}]
["Blind to suit window size 3305 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3320 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3355 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3370 x 1500mm high","m",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3390 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3400 x 1500mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3405 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3420 x 1800mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3445 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3450 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3480 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3495 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3500 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3530 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3545 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3550 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3550 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3555 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3560 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3560 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3570 x 1500mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3570 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3570 x 2100mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3600 x 2100mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3600 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3625 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3630 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3654 x 1500mm high","m",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3660 x 1200mm high","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3660 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3670 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3690 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D4189*C4189","v":{"v":0,"d":"R0.00"}}]
["Blind to suit window size 3700 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3725 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3745 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3770 x 1800mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3785 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3800 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3824 x 1200mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3830 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3840 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3855 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3890 x 1200mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3875 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3875 x 1800mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3895 x 1200mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3895 x 1500mm high","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3900 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3905 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3910 x 2400mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3915 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3915 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3920 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3920 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3970 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3990 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3990 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 3993 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 4000 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 4015 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 4050 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 4110 x 1200mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 4150 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 4153 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D4253*C4253","v":{"v":0,"d":"R0.00"}}]
["Blind to suit window size 4173 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 4190 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 4210 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 4254 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 4300 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 4310 x 1500mm wide","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 4320 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 4325 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 4330 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 4350 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 4375 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 4396 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 4400 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 4470 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 4480 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 4540 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 4555 x 1200mm high","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 4600 x 1200mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 4720 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 4735 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 4750 x 1200mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 4755 x 1200mm high","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 4765 x 1200mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 4790 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 4850 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 4992 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 5000 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 5100 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 5110 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 5128 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 5160 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 5170 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D4317*C4317","v":{"v":0,"d":"R0.00"}}]
["Blind to suit window size 5220 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 5320 x 900mm high","m",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 5360 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 5370 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 5595 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 5650 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 5700 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 5750 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 5850 x 1200mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 5850 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 5860 x 1200mm high","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 5855 x 900mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 5855 x 1800mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 5985 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 6060 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 6060 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 6160 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 6220 x 1200mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 6340 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 6520 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 6795 x 1200mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 6815 x 1200mm high","No",8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 6815 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 6850 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 7130 x 900mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blind to suit window size 7280 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["CURTAIN TRACKS, DRIP RAIL, ETC.   ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Hospi-Shadowline Cubicle Bedscreen Rails (Code SK/S21) formed of natural anodised extruded profile H/S/43353 formed to accommodate bed closures complete with 12 runners per metre and end stops fixed direct to ceiling including timber supports of 50 x 50mm pine, with and including Hospi-track bedscreen curtains (Code H/T/BSN100/9) standard height, manufactured in a poly-cotton/nylon non-iron non-stain fully washable material at a ratio of 1:25 to length of rail or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Hospital cubicle curtain track including gliders, hangers, brackets, bedscreen curtain, etc.","m",4561,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra for end plugged","No",784,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra for stop end","No",996,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra for 90° bend","No",568,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D4381*C4381","v":{"v":0,"d":"R0.00"}}]
["Extra for 45° bend","No",803,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Hospi-Slick Drip Rails CODE: H/S/DRI-3 Natural anodised (10 micron) extruded profile H/S/2897 formed in straight lengths from 1m-3m, including stop ends or similar approved. Fixed direct to ceiling including timber supports 50x50x38- SA Pine.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Drip rail","No",515,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["BATHROOM FITTINGS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke Rodan RODX611  0,8mm thick satin finished stainless steel sanitary towel disposal bin (Code: 2120070), size 200 x 295 x 165mm, plugged and screwed to the wall with stainless steel screws or similar approved ","No",451,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke Chronos BS648 satin finished stainless steel double soap dish (Code: 2120075), size 195 x 96 x 77mm high, with a deep drawn rib tray with holes, plugged and screwed to the wall with stainless steel screws or similar approved ","No",215,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke Chronos HSD Hand Sanitiser 1,2mm thick satin finished stainless steel elbow operated hand sanitiser dispenser (Code: 2120125), size 258.9 x 69.4 x 290.7mm high, plugged and screwed to the wall with stainless steel screws or similar approved ","No",75,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke CNTX70B Grade 304 18/10 satin stainless steel 32mm diameter fold away paraplegic grab rail with Franke fine grip (Code: 2510001), size 249 x 850 x 100mm deep, plugged and screwed to the wall with stainless steel screws. Installed strictly to manufacturers specification or similar approved ","No",468,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke BHM12P polished stainless steel double towel rail (Code: 2120083), size 900 x 125mm deep, plugged and screwed to the wall with stainless steel screws or similar approved ","No",120,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["800mm Long x 150mm projecting straight standard stainless steel disabled rail (IW7000). Installed strictly to manufacturers specifications. ","No",321,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Halcast anodised 251-NAT towel rail set (complete) size 450mm long with natural finish or similar approved  ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Polypropylene surface mounted horizontal baby changing station size 894mm wide x 565mm high x 589mm deep, installed strictly to manufacturers specifications (BAB001)","No",18,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke Rodan RODX600 0,8mm thick satin finished stainless steel paper towel dispenser (Code: 2120099), size 275 x 112 x 355mm high with a capacity of 500-800 towels, inspection windows on the side and Franke standard key, plugged and screwed to the wall with stainless steel screws or similar approved ","No",1335,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke Rodan RODX605 0,8mm thick satin finished stainless steel waste bin (Code: 2120097), size 355 x 168 x 460mm high with capacity of 23 litres and cylinder lock and standard Franke key, plugged and screwed to the wall with stainless steel screws or similar approved ","No",1301,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke Rodan RODX619  0,8mm thick satin finished stainless steel soap dispenser (Code: 2120095), size 200 x 85 x 140mm high with 1 litre capacity, front push button, cylinder lock and Franke standard key, plugged and screwed to the wall with stainless steel screws or similar approved ","No",1327,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke Rodan RODX672 0,8mm thick satin finished stainless steel double toilet roll holder with spindle system (Code: 2120101), size 144 x 138 x 301mm high for 2 rolls maximum 120mm diameter with cylinder lock with standard Franke key, plugged and screwed to the wall with stainless steel screws or similar approved ","No",525,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["300 x 300 x 300 x 80mm Projecting standard stainless steel dog leg side rail (IW7002). Installed strictly to manufacturers specifications.","No",457,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Masakhane shower seat with manual flip up mechanism. Frame from 25mm round steel tube with 2mm wall thickness complete with brackets for wall fixing. Seat in perforated mild steel welded to frame size 380mm W x 480mm D. Unit galvanized and painted in epoxy powder. Colour to Architect’s approval. Installed strictly to manufacturers specifications or similar approved. (San 011/011A)","No",195,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Germstar 946ml touchless dispenser with drip tray, plugged and screwed to the wall with stainless steel screws or similar approved ","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SUNDRIES","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Hat and coat hooks","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["QS Doorware stainless steel hat and coat hook (Code: QS4434) with rubber buffer or similar approved ","No",472,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Union stainless steel hat and coat hook (Code: IW5034) with rubber buffer or similar approved ","No",316,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Union 500m long aluminium multi rack with four hooks (Code AL8101AS) installed strictly to manufacturers specifications or similar approved. (HK001/HK001A)","No",231,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Wall mounted hook installed strictly to manufacturers specifications, (HK009)","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Broom and mop hook","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Purpose made back plate to be 900 x 450mm high non magnetic 1.6mm stainless steel plate with grid 180 satin finish, glued and screwed (with wall plugs) to a wall surface, with an approved adhesive and six countersunk stainless steel screws, complete with standard stainless steel wall rail - 900mm long with five broom hooks (HK005)","No",36,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["DRUG CABINET","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Standard 711 x 280 x 762/711mm high lockable mild steel drug cabinet complete with internal lockable compartment and shelves Type D with PPA 200 Micron coat finish all to comply with SABS standards. Colour to Architects Approval  all in accordance with annexed drug cabinet specification HDG-100-R Drug cabinet specification","No",35,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["INSTRUMENT CABINET","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,6mm Stainless steel Grade 304 (18/10) or similar approved ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,6mm Grade 304 18/10 stainless steel instrument cabinet (Code: 359630), size 900 x 300 x 600mm with 2No. doors fitted with shatterproof glass panels, 2No. shelves,  Cam lock with 2No. keys bolted to wall with M6 stainless steel expanding bolts (CUPW029)","No",47,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D4445*C4445","v":{"v":0,"d":"R0.00"}}]
["Franke 1,6mm Grade 304 18/10 stainless steel instrument cabinet (Code: 2630063), size 900 x 300 x 600mm with 2No. doors fitted with shatterproof glass panels, Cam lock with 2No. keys and 2No. shelves, bolted to wall with M6 stainless steel expanding bolts.","No",46,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["STAINLESS STEEL INSTRUMENT CABINET","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["1,6mm Grade 304 18/10 stainless steel instrument cabinet size 900 x 300 x 600mm (no doors) including  2No. shelves, bolted to wall with M6 stainless steel expanding bolts. All to comply with SABS standards and as per Architect details","No",18,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["1,6mm Grade 304 18/10 stainless steel instrument cabinet size 900 x 300 x 600mm including 2No. doors (equal size) fitted with shatterproof glass panels including cam lock with 2No. keys and 2No. shelves, bolted to wall with M6 stainless steel expanding bolts. All to comply with SABS standards and as per 100-G-Joinery schedule from HDG","No",16,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["KEY CABINET","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Saunderson Security (0800 204 563) or similar approved ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Wall mounted standard Fortis key cabinet with 100 hooks size 540 x 420 x 55mm deep (CUP001)","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["GUN SAFE","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Austen Security Safes (012 803 0689) or similar approved ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Gun safe, model WS3 (colour dove grey) size overall  330 x 305 x 300mm deep, bolted into position with expansion bolts. (SAF001)","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Tactical distributors SA (011 823 2401) or similar approved ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["BTP bullet trap (SAF004)","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["STAINLESS STEEL TABLES, BENCH, CABINET, ETC.","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Stainless steel Grade 304 (18/10) or similar approved ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 800 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet and a set of 38mm diameter stainless steel detachable legs with adjustable flanged foot pieces","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 900 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet and a set of 38mm diameter stainless steel detachable legs with adjustable flanged foot pieces","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 1000 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet and a set of 38mm diameter stainless steel detachable legs with adjustable flanged foot pieces","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 1100 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet and a set of 38mm diameter stainless steel detachable legs with adjustable flanged foot pieces","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 1250 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet and a set of 38mm diameter stainless steel detachable legs with adjustable flanged foot pieces","No",8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 1300 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet and a set of 38mm diameter stainless steel detachable legs with adjustable flanged foot pieces","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 1400 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet and a set of 38mm diameter stainless steel detachable legs with adjustable flanged foot pieces","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 1500 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet and a set of 38mm diameter stainless steel detachable legs with adjustable flanged foot pieces","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 1600 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet and a set of 38mm diameter stainless steel detachable legs with adjustable flanged foot pieces","No",8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 1700 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet and a set of 38mm diameter stainless steel detachable legs with adjustable flanged foot pieces","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 1800 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet and a set of 38mm diameter stainless steel detachable legs with adjustable flanged foot pieces","No",21,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 1900 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet and a set of 38mm diameter stainless steel detachable legs with adjustable flanged foot pieces","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 2000 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet and a set of 38mm diameter stainless steel detachable legs with adjustable flanged foot pieces","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 2100 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet and a set of 38mm diameter stainless steel detachable legs with adjustable flanged foot pieces","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 2200 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet and a set of 38mm diameter stainless steel detachable legs with adjustable flanged foot pieces","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 2400 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet and a set of 38mm diameter stainless steel detachable legs with adjustable flanged foot pieces","No",7,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 2600 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet and a set of 38mm diameter stainless steel detachable legs with adjustable flanged foot pieces","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 2700 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet and a set of 38mm diameter stainless steel detachable legs with adjustable flanged foot pieces","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D4509*C4509","v":{"v":0,"d":"R0.00"}}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 2800 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet and a set of 38mm diameter stainless steel detachable legs with adjustable flanged foot pieces","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 2900 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet and a set of 38mm diameter stainless steel detachable legs with adjustable flanged foot pieces","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 3000 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet and a set of 38mm diameter stainless steel detachable legs with adjustable flanged foot pieces","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 3150 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet and a set of 38mm diameter stainless steel detachable legs with adjustable flanged foot pieces","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 3500 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet and a set of 38mm diameter stainless steel detachable legs with adjustable flanged foot pieces","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 3600 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet and a set of 38mm diameter stainless steel detachable legs with adjustable flanged foot pieces","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 4000 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet and a set of 38mm diameter stainless steel detachable legs with adjustable flanged foot pieces","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 4100 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet and a set of 38mm diameter stainless steel detachable legs with adjustable flanged foot pieces","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 4400 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet and a set of 38mm diameter stainless steel detachable legs with adjustable flanged foot pieces","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 4500 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet and a set of 38mm diameter stainless steel detachable legs with adjustable flanged foot pieces","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 6000 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet and a set of 38mm diameter stainless steel detachable legs with adjustable flanged foot pieces","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 6700 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet and a set of 38mm diameter stainless steel detachable legs with adjustable flanged foot pieces","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 900 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet ","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 1000 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 1300 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 1400 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet ","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 1500 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet ","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 1600 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 1700 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet ","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 1800 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 1900 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 2000 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet ","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 2100 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet ","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 2200 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 2300 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 2400 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet ","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 2500 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet ","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 2600 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet ","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 2700 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 2800 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 2900 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 3000 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet ","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D4573*C4573","v":{"v":0,"d":"R0.00"}}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 3100 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 3200 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 3400 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 3600 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet ","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 3800 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 4200 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet ","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 4400 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 4800 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 4900 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 510 x  650 x 1050mm with 150mm high integral splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 2000 x  600 x 1050mm without splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 2500 x  600 x 1050mm without splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet ","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 2700 x  600 x 1050mm without splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 2900 x  600 x 1050mm without splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 3600 x  600 x 1050mm without splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 purpose made stainless steel W wall bench size 3700 x  600 x 1050mm without splashback to rear, 50 x 10mm turndown, underside sprayed with vermin proof bitumastic sound deadening and supported on 30 x 30 x 3mm painted mild angle framework with galvanised mild steel backing sheet ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["WRITING BOARDS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Purpose made white boards by Parrot Products, installed complete under a two year written guarantee or similar approved ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["White patient name and bed number writing board 250 x 270mm high with printed lettering according to detailed drawing (HDG-046-008), installed strictly to manufacturer's specifications (BOA023)","No",415,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["White writing board 600 x 1000mm high with printed lettering according to drawings and installed strictly to manufacturer's specifications (BOA001)","No",248,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["White writing board 1200 x 1000mm high with printed lettering according to detailed drawing (HDG-046-007) installed strictly to manufacturer's specifications (BOA021)","No",14,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["White writing board 1500 x 1000mm high with printed lettering according to detailed drawing (HDG-046-005-block no.) installed strictly to manufacturer's specifications (BOA004A)","No",11,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["White writing board 1500 x 1000mm high with printed lettering according to detailed drawing (HDG-046-006) installed strictly to manufacturer's specifications (BOA020)","No",14,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PINNING BOARDS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Pin boards with carpet to pinning board by Parrot Products installed complete under a two year written guarantee or similar approved ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Standard 600mm x 1000mm pin board all installed strictly to manufacturer’s specifications, plugged (BOA009)","No",253,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Standard 1000mm x 1000mm pin board all installed strictly to manufacturer’s specifications, plugged (BOA010)","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PROJECTOR SCREEN","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Standard projector screen complete with ceiling box","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Standard 1760 x 1330mm projector screen, all installed strictly to manufacturer's specifications (SCR004)","No",11,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["X-RAY VIEWING SCREENS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["X-ray viewing screens by HUTZ or similar approved ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D4637*C4637","v":{"v":0,"d":"R0.00"}}]
["Standard single surface mount single X-ray viewing screen size 360 x 429 and 1 plate, complete with switch and fluorescent lamps (HU-XRU-W-01). Installed strictly to manufacturers specifications (ILL001-EE)","No",108,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Standard single surface mount single X-ray viewing screen size 960 x 429 with 2 plates, complete with switch and fluorescent lamps (HU-XRU-W-02). Installed strictly to manufacturers specifications (ILL002-EE)","No",37,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["GLOVE, CAPS AN MASKS DISPENSER","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ingwe metal craft or similar approved ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Purpose made protection system dispensing IPS consumables, dispenser to hold flat pack or launderable gowns, two boxes of gloves and one box of ear loop face masks and one box caps with cylinder lock with standard key, plugged and screwed to the wall with stainless steel screws","No",72,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["VANDAL RESISTANT FURNITURE","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cranium Medical Products or similar approved ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["4 Seater Stainless steel table that can be used in recreational or dining areas.  (PSY015)","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["STEEL LOCKERS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ingwe metal craft lockers or similar approved ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Standard x3 PPA 200 micron coated two tier change lockers, complete with one PPA 200 micron coated mild steel sit bench unit with perforated bench. Installed strictly to manufacturers specifications (LOC002)","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Standard x3 PPA 200 micron coated two tier change lockers. Installed strictly to manufacturers specifications (LOC003)","No",341,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Standard 4 drawer powder coated mild steel filing cabinet complete with locking mechanism. Installed strictly to manufacturers specifications (CupF023)","No",109,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["MODULAR STEEL SHELVING, RAILS, BINS, ETC.","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ingwe metal craft modular shelving or similar approved ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Standard 550 x 246mm utility shelf with PPA 200 micron finish complete with wall supports (SH015)","No",234,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Standard clothing rail complete with wall brackets with PPA MICRON finish, installed to manufacturers specification (SH016)","No",46,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Standard 1500 X 1800mm high PPA MICRON wall louvre panel complete with 32 lin bin combination, installed to manufacturers specification (SH018)","No",77,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Standard 1050 x 610mm  high PPA 200 MICRON wall rail complete with 30 LinBin combination (x9/size2, x9/size3, x12/size5) (LB-30) (SH046)","No",168,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Purpose made 1100 X 246 utility shelf complete with wall supports with PPA 200 MICRON finish (USNC – 5/2/1T) (SH055)","No",184,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Store Direct (011 608 0250) or similar approved ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Standard double sided free-standing panel 1400 x 1500 with 120 colour Linbins (code: STRPK12) (SH059)","No",11,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Tidy Files (011 943 4210) or similar approved ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Standard modular Push Pull Bulk Filer shelving, size 914 x 381 x 2210mm high with 5x mid-shelves combined into single stationary wall end/sliding open end shelf as indicated in individual rooms (SH039)","No",22,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Standard modular Push Pull Bulk Filer shelving, size 914 x 381 x 2210mm high with 5x mid-shelves combined into single stationary wall end/sliding open end shelf as indicated in individual rooms (SH040)","No",27,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Standard modular Push Pull Bulk Filer shelving, size 914 x 381 x 2210mm high with 5x mid-shelves combined into double sliding shelf as indicated in individual rooms (SH041)","No",32,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Standard modular Push Pull Bulk Filer shelving, size 914 x 381 x 2210mm high with 5x mid-shelves combined into double sliding shelf as indicated in individual rooms (SH042)","No",31,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Krost modular shelving or similar approved ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["914 x 381 x 1905mm High 5 tier slatted shelf unit bolted to ground, with bracing strips (SH065)","No",19,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["914 x 457 x 1905mm High 5 tier slatted shelf unit bolted to ground, with bracing strips (SH066)","No",663,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["914 x 610 x 1905mm High 5 tier slatted shelf unit bolted to ground, with bracing strips (SH067)","No",349,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["914 x 381 x 1905mm High 5 tier solid shelf unit bolted to ground, with bracing strips (SH068)","No",96,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D4701*C4701","v":{"v":0,"d":"R0.00"}}]
["914 x 457 x 1905mm High 5 tier solid shelf unit bolted to ground, with bracing strips (SH069)","No",691,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["914 x 610 x 1905mm High 5 tier solid shelf unit bolted to ground, with bracing strips (SH070)","No",165,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["2100 x 500 x 2100mm High Standard PPA 200 MICRON coated 3 tier heavy duty shelf unit (HD-2.7/5/2/3T) (SH031C)","No",165,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["2100 x 1000 x 2100mm High Standard PPA 200 MICRON coated 3 tier heavy duty shelf unit (HD-2.7/5/2/3T)  (SH032C)","No",69,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["610-457mm Wall mounted 4 tier slatted shelving (SH071)","m",169,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["BENCHES, ETC.","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Airport seating with one piece seat shell in 2mm thick perforated stainless steel grade 430 brushed finish, supported by a full framework in 6mm thick laser cut mild steel, complete with round cross bars in stainless steel. Chairs mounted on a steel beam with 3mm wall thickness without armrests. Leg pieces on extreme ends of unit in 10mm laser cut mild steel","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Two seater bench configuration, size 900mm high x 600mm deep x 1100mm wide, installed to floor, strictly to manufacturers specifications (CHA023)","No",26,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Three seater bench configuration, size 900mm high x 600mm deep x 1700mm wide, installed to floor, strictly to manufacturers specifications (CHA024)","No",169,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Four seater bench configuration, size 900mm high x 600mm deep x 2300mm wide, installed to floor, strictly to manufacturers specifications (CHA025)","No",126,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Five seater bench configuration, size 900mm high x 600mm deep x 2900mm wide, installed to floor, strictly to manufacturers specifications (CHA026)","No",113,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cubicle Solutions (086 100 0451) Integrated Upstand bench (Code: CSBEN/chpl), comprising powder coated mild steel frame with 12mm thick compact high pressure laminate slated seat and backrest pop-riveted to frame with grade 304 stainless steel hat and coat hooks (Code: CSSH&C02/304) or similar approved, strictly to manufacturers specifications.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["450 x 1200 x 1810mm Long Integrated Upstand bench (CUB002)","No",19,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PANEL HEATERS, ETC.","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Panel Heater by SALTON  model No: SPH55-N or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["600 x 600 x 11mm thick panel heater, installed strictly according manufacturer's specifications (PAN001)","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PALLET, ETC.","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Plastic Pallets by Ingwe Metal Craft  (083 377 1919) or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Standard 1000 x 1200mm Plastic pallet (Code PP-1/1.2) installed strictly according manufacturer's specifications (PLT001)","No",46,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["LETTERS, NAMEPLATES, ETC. (PROVISIONAL)","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["In accordance with \"Limpopo Central Hospital - Sign Schedule\" dated June 2021, Rev 1.11.0","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Customized ","H4",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fabricated Name and Logo Exterior Signs",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Wall Mounted",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["8mm Thick aluminium fabricated name sign with overall size 12 452 x 788.5mm high consisting of several letters, complete (Type LCH2) (Limpopo Central Hospital)","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SIGNAGE (PROVISIONAL)","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["In accordance with \"Limpopo Central Hospital - Sign Schedule\" dated June 2021, Rev 1.11.0","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Vista Expand System or similar approved ","H4",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Municipal Road Signs",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Floor Mounted ",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clear anodised aluminium double sided post and pylon sign with overall size 2318 x 2509mm high, complete (Type LCH1)","No",10,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Vista Light System or similar approved ","H4",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D4765*C4765","v":{"v":0,"d":"R0.00"}}]
["Emergency Signs",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Wall Mounted ",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clear anodised aluminium curved single sided wall frame sign with overall size 3003 x 1332mm high, complete (Type LCH3)","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Vista System or similar approved ","H4",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Directional Signs",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Floor Mounted ",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clear anodised aluminium curved double sided pylon sign with overall size 606.2 x 1989mm high, complete (Type LCH6)","No",12,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clear anodised aluminium curved double sided pylon sign with overall size 818.5 x 2013mm high, complete (Type LCH5)","No",8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clear anodised aluminium curved double sided pylon sign with overall size 1017.3 x 3013mm high with and including sign holder extrusions with overall size 1017.3 x 1543mm high, complete (Type LCH4)","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clear anodised aluminium curved double sided post and pylon sign with overall size 606.2 x 1812mm high, complete (Type LCH7)","No",8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Aluminium curved double sided pylon sign with overall size 650 x 1812mm high, complete (Type LCH8)","No",14,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Wall Mounted",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clear anodised aluminium curved single sided sign with overall size 606.2 x 1213mm high with and including sign holder extrusions with overall size 606.2 x 1213mm high, complete (Type LCH9)","No",75,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sections, Intersections, Bed Numbers and Door Signs",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Door Mounted",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clear anodised aluminium curved single sided wall frame sign with overall size 493 x 151mm high, complete (Type LCH10)","No",2198,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clear anodised aluminium curved single sided wall frame sign with overall size 216 x 205mm high, complete (Type LCH14)","No",400,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Wall Mounted",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clear anodised aluminium curved single sided wall frame sign with overall size 506.5 x 215mm high, complete (Type LCH11)","No",87,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clear anodised aluminium curved single sided wall frame sign with overall size 101 x 105.2mm high, complete (Type LCH15)","No",688,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Wall Projected ",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clear anodised aluminium curved double sided projected signs with overall size 252.3 x 303mm high, complete (Type LCH13)","No",200,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Suspended from Ceilings and or Roofs",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clear anodised aluminium curved double sided two-tier signs with overall size 614 x 206.5mm high, complete (Type LCH12)","No",189,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sundries","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Vinyl decals applied on above signage (Wording of departments, wards, toilets, etc.) ","m2",454,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["FIRE SIGNAGE (PROVISIONAL)","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["190 x 190mm High photo luminescent fire signage as per fire consultants drawings","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Wall Mounted","H4",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Escape route signage (Code: E9)","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Escape route signage (Code: E15)","No",11,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Wheelchair signage (Code: GA22)","No",24,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D4829*C4829","v":{"v":0,"d":"R0.00"}}]
["190 x 380mm High photo luminescent fire signage as per fire consultants drawings","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Wall Mounted","H4",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Escape route signage (Code: E1)","No",13,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Escape route signage (Code: E2)","No",13,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Escape route signage (Code: E3)","No",630,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Escape route signage (Code: E13) Chromadek","No",12,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fire equipment signage (Code: F13)","No",137,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fire equipment signage (Code: F15)","No",47,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fire equipment signage (Code: F45) Chromadek","No",10,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Suspended from Ceilings and or Roofs","H4",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Escape route signage (Code: E1)","No",86,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Escape route signage (Code: E2)","No",103,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Escape route signage (Code: E3)","No",87,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Escape route signage (Code: E13)","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fire equipment signage (Code: F16)","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fire equipment signage (Code: F16/F19) back to back signs","No",15,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fire equipment signage (Code: F19)","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Escape route signage (Code: E1/E2) back to back signs","No",320,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Escape route signage (Code: E2/E3) back to back signs","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Escape route signage (Code: E3/E3) back to back signs","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["190 x 570mm High photo luminescent fire signage as per fire consultants drawings","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Wall Mounted","H4",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fire equipment signage (Code: F4)","No",136,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fire equipment signage (Code: F5)","No",8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fire equipment signage (Code: F6)","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Escape route signage (Code: E17)","No",9,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Escape route signage (Code: E19)","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Escape route signage (Code: E18) Chromadek","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Suspended from Ceilings and or Roofs","H4",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fire equipment signage (Code: F4)","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fire equipment signage (Code: F5)","No",24,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fire equipment signage (Code: F6)","No",11,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D4893*C4893","v":{"v":0,"d":"R0.00"}}]
["Fire equipment signage (Code: F5/F6) back to back signs","No",154,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Escape route signage (Code: E16/E19) back to back signs","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Escape route signage (Code: E16/E17) back to back signs","No",12,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["190 x 760mm High photo luminescent fire signage as per fire consultants drawings","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Wall Mounted","H4",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fire equipment signage (Code: F1)","No",114,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Suspended from Ceilings and or Roofs","H4",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fire equipment signage (Code: F2)","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fire equipment signage (Code: F2/F3)","No",105,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fire equipment signage (Code: F3)","No",15,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TOTAL IRONMONGERY",null,0,null,{"$f":"SUM(E3079:E4913)","v":{"v":0,"d":"0.00"}}]
[null,null,0,null,{"v":0,"d":"R0.00"}]
["SECTION 2","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NEW HOSPITAL ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["BILL NO 10","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["STRUCTURAL STEELWORK ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PREAMBLES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Preambles for Trades as defined in Scope of Work (C3.1 Item 4.1 & Item 4.2)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TRADE NAMES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Any reference to trade names in the Bills of Quantities or  Architect's specification or drawings shall deem to mean \"or similar and approved\"",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SUPPLEMENTARY PREAMBLES","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Descriptions of bolts shall be deemed to include nuts and washers ",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Descriptions of L shaped and U-shaped anchor bolts shall be deemed to include bending, threading, nuts and washers and embedding in concrete",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Descriptions of expansion anchors and bolts and chemical anchors and bolts shall be deemed to include nuts, washers and mortices in brickwork or concrete ____________________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 134 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["WORKSHOP DRAWINGS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Preparation of all workshop drawings for approval by Principal Agent before manufacturing","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["MILD STEEL","H1",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The following in welded and bolted roof trusses, erected approximately 3.5m above floor level ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Angle sections, flat sections, etc. in tie beams, rafters, struts, bracing, etc. of roof trusses","t",64.88,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["I sections, IPE sections, etc. in tie beams, rafters, struts, bracing, etc. of roof trusses","t",64.59,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Angle sections, flat sections, etc. in brackets, base plates,  connector plates, etc. ","t",12.87,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The following in welded and bolted roof trusses, erected approximately 4.5m above floor level ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D4957*C4957","v":{"v":0,"d":"R0.00"}}]
["Angle sections, flat sections, etc. in tie beams, rafters, struts, bracing, etc. of roof trusses","t",6.99,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["I sections, IPE sections, etc. in tie beams, rafters, struts, bracing, etc. of roof trusses","t",6.96,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Angle sections, flat sections, etc. in brackets, base plates,  connector plates, etc. ","t",1.39,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The following in welded and bolted roof trusses, erected approximately 8m above floor level ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Angle sections, flat sections, etc. in tie beams, rafters, struts, bracing, etc. of roof trusses","t",18.06,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["I sections, IPE sections, etc. in tie beams, rafters, struts, bracing, etc. of roof trusses","t",17.98,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Angle sections, flat sections, etc. in brackets, base plates,  connector plates, etc. ","t",3.58,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The following in welded and bolted roof trusses, erected approximately 12.5m above floor level ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Angle sections, flat sections, etc. in tie beams, rafters, struts, bracing, etc. of roof trusses","t",42.38,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["I sections, IPE sections, etc. in tie beams, rafters, struts, bracing, etc. of roof trusses","t",42.19,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Angle sections, flat sections, etc. in brackets, base plates,  connector plates, etc. ","t",8.41,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The following in welded and bolted roof trusses, erected approximately 13.5m above floor level ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Angle sections, flat sections, etc. in tie beams, rafters, struts, bracing, etc. of roof trusses","t",18.76,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["I sections, IPE sections, etc. in tie beams, rafters, struts, bracing, etc. of roof trusses","t",18.68,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Angle sections, flat sections, etc. in brackets, base plates,  connector plates, etc. ","t",3.72,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The following in welded and bolted roof trusses, erected approximately 16.5m above floor level ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Angle sections, flat sections, etc. in tie beams, rafters, struts, bracing, etc. of roof trusses","t",98.13,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["I sections, IPE sections, etc. in tie beams, rafters, struts, bracing, etc. of roof trusses","t",97.69,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Angle sections, flat sections, etc. in brackets, base plates,  connector plates, etc. ","t",19.47,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Welded beams, purlins, bracing, etc.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cold formed lipped channel in purlins, etc.","t",127.2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cold formed lipped channel in cladding rails, etc.","t",12.9,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Angle sections, flat sections, etc. in brackets, base plates,  connector plates, etc. ","t",12.37,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The following in welded and bolted steel columns and beams","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["I-section and H-section columns and beams","t",115.32,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Tubular section beam","t",6.41,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Angle sections in bracing, etc.","t",32.03,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Angle sections, flat sections, etc. in brackets, base plates,  connector plates, etc.","t",4.81,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PLANTROOMS ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The following in welded and bolted steel columns and beams ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Vital Engineering Vitagrid pressure forged VE40Z modular walkway panel with 25 x 45mm serrated non-slip bearer bars in galvanised mild steel including banding on all sides or similar approved, laid in mild steel angle (elsewhere measured)","m2",1378,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["I-section and H-section columns and beams","t",78.59,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D5021*C5021","v":{"v":0,"d":"R0.00"}}]
["Angle sections in bracing, etc.","t",35.13,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Angle sections, flat sections, etc. in brackets, base plates,  connector plates, etc.","t",8.27,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["GALVANISED STEEL ","H1",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The following in welded and bolted galvanised canopies, erected approximately 4.5m above floor level ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["I sections, IPE sections, etc. in tie beams, rafters, struts, bracing, etc. ","t",2.4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Rectangular hollow section beams","t",3.38,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Tubular section in tie beams, rafters, struts, bracing, etc. of roof trusses","t",2.16,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Angle sections, flat sections, etc. in brackets, base plates,  connector plates, etc.","t",1.08,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The following in galvanised welded purlins, bracing, sag rods, gusset plates, etc. bolted to steel structure, etc.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Rectangular hollow section purlins ","t",2.47,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Gutters ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["2mm Thick welded galvanised steel rainwater gutter 600mm girth, welded to form slope at bottom, four times bent and fixed to purlins, including painting inside with epoxy tar, welding complete","m",71,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over for stop end","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["COURTYARD WALKWAYS ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The following in galvanised stringers, sections, vastraps, etc. ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Vital Engineering Vitagrid pressure forged VE100Z modular walkway panel with 25 x 45mm serrated non-slip bearer bars in galvanised mild steel including banding on all sides or similar approved, loose laid in mild steel angle (elsewhere measured)","m2",2313,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Rectangular hollow section beams","t",30.65,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Angle sections ","t",15.62,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Angle sections, flat sections, etc. in brackets, base plates,  connector plates, etc.","t",1.8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Chemical bolts","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["M16 ChemIcal anchor bolts","No",2286,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TRENCH COVERS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The following in galvanised stringers, sections, vastraps, etc. ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Vital Engineering Vitagrid pressure forged VE40Z modular walkway panel with 25 x 45mm serrated non-slip bearer bars in galvanised mild steel including banding on all sides or similar approved, loose laid in mild steel angle (elsewhere measured)","m2",369,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Angle sections ","t",2.15,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Flat bar in lugs","t",0.09,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["BOLTS, FASTENERS, ETC","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["M16 ChemIcal anchor bolts","No",2106,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["M22 ChemIcal anchor bolts","No",702,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["BUDGETARY ALLOWANCES ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow the Amount of R600 000.00 (Six Hundred Thousand Rand) for Catladders and Catwalks to be used at the discretion of the Employer, or to be deducted in whole or in part if not required","Item",1,{"v":600000,"d":"R600,000.00"},{"v":600000,"d":"R600,000.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TOTAL STRUCTURAL STEELWORK ",null,0,null,{"$f":"SUM(E4934:E5083)","v":{"v":600000,"d":"600,000.00"}}]
[null,null,0,null,{"v":0,"d":"R0.00"}]
["SECTION 2","H2",0,null,{"$f":"D5086*C5086","v":{"v":0,"d":"R0.00"}}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NEW HOSPITAL ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["BILL NO 11","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["METALWORK ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PREAMBLES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Preambles for Trades as defined in Scope of Work (C3.1 Item 4.1 & Item 4.2)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TRADE NAMES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Any reference to trade names in the Bills of Quantities or  Architect's specification or drawings shall deem to mean \"or similar and approved\"",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["DETAIL DESCRIPTION AND SPECIFICATION","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Annotations at end of description i.e. (D01) refer to the Architect's specification attached to the back of these bills of quantities. Tenderers are advised to study the Architect's specification for the full intent and meaning of the relevant item",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SUPPLEMENTARY PREAMBLES","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Descriptions","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Descriptions of bolts shall be deemed to include nuts and washers  Descriptions of expansion anchors and bolts and chemical anchors and bolts shall be deemed to include nuts, washers and mortices in brickwork or concrete  Metalwork described as \"holed for bolt(s)\" shall be deemed to exclude the bolts unless otherwise described ____________________",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: All stainless steel members to be manufactured with grade 316 stainless steel complete with grid 180 satin finish","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 136 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["HANDRAILS, BALUSTRADES.","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Type 1 Epoxy powder coated welded mild steel balustrade overall 1000mm high, comprising one 1.5mm x 50mm diameter pipe handrail,  12 x 40mm flat bar top and bottom rail and 12 x 40mm flat bar balusters at 103mm centres including 12mm rod on 12 x 40mm flat bar posts at 1,2m centres and fixed to floor by core drilling into concrete and epoxy grouting posts into concrete including 12 x 40mm mild steel spacers (Refer to Drawings 040-050 and TYP-042-026 at the back of these Bills of Quantities)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Balustrade fixed to concrete ","m",615,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Raking balustrade fixed to concrete ","m",465,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over 50mm diameter top rail for closed end","No",160,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over for mitred angle","No",292,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over for ramp or knee","No",395,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Type 3 Epoxy powder coated welded mild steel handrail fixed 128mm high above brick balustrade wall, comprising a 50mm diameter 1.5mm thick steel pipe with and including 12 x 40mm flat bar posts 122mm high and 120 x 68 x 6mm thick flange plate fix to wall at 1.2m centres with two 10mm diameter expansion bolts (Refer to Drawing 040-052 at the back of these Bills of Quantities)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Handrail fixed to top of walls","m",423,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but circular on plan","m",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Raking handrail fixed to walls","m",66,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over for closed end ","No",144,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over for ramp or knee","No",17,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over for mitred angle","No",7,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Type 4 Epoxy powder coated welded mild steel balustrade overall 1137mm high, comprising 10mm thick double profiled steel post assembly, one 1.5mm x 50mm diameter pipe handrail and one bottom rail,  12 mm diameter top and bottom track and balusters at 105mm centres and fixed to structural steel members (Refer to Drawings 040-053 at the back of these Bills of Quantities)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Balustrade fixed to steel","m",445,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Raking balustrade fixed to steel","m",33,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D5149*C5149","v":{"v":0,"d":"R0.00"}}]
["Balustrade fixed to concrete","m",16,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but circular on plan","m",21,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but helical","m",26,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over 50mm diameter top and bottom rail for closed end","No",32,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over for mitred angle","No",38,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over for ramp or knee","No",25,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Type 10 Epoxy powder coated welded mild steel handrail fixed to walls, comprising a 50mm diameter 1.5mm thick steel pipe with and including 12 mm diameter once bent round bar bracket approximately 65mm girth and 120 x 50 x 4mm thick flange plate fixed to wall at 1.2m centres with two 10mm diameter expansion bolts (Refer to Drawing 040-059 at the back of these Bills of Quantities)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Handrail fixed to walls","m",401,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Raking handrail fixed to walls","m",441,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over for closed end ","No",183,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over for mitred angle","No",57,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over for ramp or knee","No",307,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Type 2 Welded hot dipped galvanised steel balustrade overall 745mm high, comprising one 1.5mm x 50mm diameter pipe handrail,  12 x 40mm flat bar top and bottom rail and 12 x 40mm flat bar balusters at 103mm centres on 12 x 40mm flat bar posts at 1,2m centres and fixed to floor by core drilling into concrete and epoxy grouting posts into concrete including 12 x 40mm mild steel spacers (Refer to Drawings 040-051 and TYP-042-026 at the back of these Bills of Quantities)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Balustrade fixed to concrete ","m",382,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Raking balustrade fixed to concrete ","m",18,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over 50mm diameter top rail for closed end","No",103,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over for mitred angle","No",31,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over for ramp or knee","No",31,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Type 5 Welded hot dipped galvanised steel handrail fixed to walls, comprising a 50mm diameter 1.5mm thick steel pipe with and including 12 mm diameter once bent round bar bracket approximately 65mm girth and 120 x 50 x 4mm thick flange plate fixed to wall at 1.2m centres with two 10mm diameter expansion bolts (Refer to Drawing 040-054 at the back of these Bills of Quantities)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Handrail fixed to walls","m",118,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Raking handrail fixed to walls","m",222,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but circular on plan","m",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over for closed end ","No",73,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over for mitred angle","No",34,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over for ramp or knee","No",102,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Type 11 Welded hot dipped galvanised steel handrail fixed to aluminium,  comprising a 50mm diameter 1.5mm thick steel pipe with and including 12 mm diameter round bar bracket approximately 41mm long and 100 x 50 x 4mm thick flange plate fixed to columns at 1.2m centres with two pop rivets (Refer to Drawing 040-060 at the back of these Bills of Quantities)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Handrail fixed to walls","m",353,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over for closed end ","No",48,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Type 6 Vital Engineering Maclock medium duty or similar approved hot dipped galvanised epoxy powder coated safety railing  fixed to floor by core drilling into concrete and epoxy grouting into concrete (Refer to Drawing 040-055 at the back of these Bills of Quantities) Installed strictly in accordance with the manufacturer's specifications.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Balustrade fixed to concrete ","m",367,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Raking balustrade fixed to concrete","m",205,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over for closed end","No",65,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D5213*C5213","v":{"v":0,"d":"R0.00"}}]
["Extra over for mitred angle","No",36,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over for ramp or knee","No",23,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Type 7 Vital Engineering Maclock medium duty or similar approved hot dipped galvanised epoxy powder coated safety railing  fixed to steel with wall plates (Refer to Drawing 040-056 at the back of these Bills of Quantities) Installed strictly in accordance with the manufacturer's specifications.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Balustrade fixed to concrete ","m",2458,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over for closed end","No",204,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over for mitred angle","No",255,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Type 8 Welded hot dipped galvanised steel handrail fixed to walls, comprising a 50mm diameter 1.5mm thick steel pipe with and including 12 mm diameter round bar bracket approximately 41mm long and 120 x 50 x 4mm thick flange plate fixed to wall at 1.2m centres with two 10mm diameter expansion bolts (Refer to Drawing 040-057 at the back of these Bills of Quantities)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Handrail fixed to walls","m",504,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but circular on plan","m",75,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Raking handrail fixed to walls","m",1201,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over for closed end ","No",32,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over for mitred angle","No",34,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over for ramp or knee","No",364,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Type 9 Welded stainless steel proprietary handrail fixed 1000mm above floor level, comprising a 50.8mm diameter stainless steel pipe with groove for LED strip lighting including 12.7mm stainless steel rod and 50mm diameter stainless steel wall flange fixed to wall at 1.5m intervals. Refer to (Detail 040-061)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Handrail fixed to walls","m",20,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Raking handrail fixed to walls","m",31,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over for closed end ","No",8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over for mitred angle","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over for ramp or knee","No",11,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Welded stainless steel handrail fixed 900mm above floor level, comprising a 50mm diameter 1.5mm thick stainless steel pipe including 12mm stainless steel rod and 30 x 50 x 2mm thick stainless steel wall flange to fix handrail to wall with two stainless steel pop rivets at 1.5m intervals. Refer to (Detail 040-DT12) BUM009","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Handrail fixed to walls","m",369,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over closed end ","No",142,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Purpose made 50mm diameter 1.5mm thick stainless steel bumper rail complete with end caps including reveal and 12mm diameter stainless steel rod wall pin and 50mm diameter wall flange at maximum 500mm centres. Fixed with 6 x 60mm long coach screw with heavy duty wall plugs including approved epoxy grout 875mm above finished floor level. Purpose made 50mm diameter 1.5mm thick stainless steel bumper rail complete with end caps including reveal and 12mm diameter stainless steel rod wall pin and 50mm diameter wall flange at maximum 500mm centres. Fixed with 6 x 60mm long coach screw with heavy duty wall plugs including approved epoxy grout 700mm above finished floor level. All bolts, washers nuts, screws etc. to be corrosion proof. All installed strictly to manufacturers specifications. Refer to (Detail 040-DT13) BUM010","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Double wall guard fixed to wall","m",16,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over for stop ends, etc. ","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["WIREFORCE SECURITY FENCING SYSTEM","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Zinc Aluminium Polyester Powder coated Securemax 3510 fencing system including fencing posts, cover plates, base plates, caps, etc. complete or similar approved. All in accordance with the manufacturer's instructions","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fence 2000mm high","m",11,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fence 2100mm high","m",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fence 2400mm high","m",200,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fence 3000mm high","m",135,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over 2400mm high fence for single gate 900mm wide","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D5277*C5277","v":{"v":0,"d":"R0.00"}}]
["Extra over 2400mm high fence for double gate 1800mm wide","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Galvanised mild steel flattened expanded metal panels (Flatex 358/VEM6315F) or similar approved, clamped between steel sections (measured elsewhere)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Galvanized welded expanded metal mesh ","m2",505,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["MINOR STEEL WORK","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The following in welded and bolted steel columns ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["75 x 75 x 3mm Square hollow section column in mullions","m",140,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Angle sections, flat sections, etc. in brackets, base plates,  connector plates, etc. ","t",0.34,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["M16 ChemIcal anchor bolts","No",352,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The following in welded and bolted steel cornice ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["60 x 60 x 3mm Angle section fixed to slab soffit ","m",1361,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["20 x 20 x 2mm Angle section welded to steel angle ","m",1361,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["MINOR GALVANISED MILD STEEL WORK","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The following in wall stiffeners to brickwork","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["90 x 90 x 8mm Plate wall stiffeners suitable for half brick walls with and including 60 x 60 x 6 angle 100mm long welded all round to plates at top and bottom, bolted to slabs with and including 16mm diameter chemical anchors, all as per engineer's standard detail","No",150,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["200 x 90 x 8mm PL wall stiffeners suitable for one brick walls with and including 60 x 60 x 6 angle 100mm long welded all round to plates at top and bottom, bolted to slabs with and including 16mm diameter chemical anchors, all as per engineer's standard detail","No",350,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["MINOR STAINLESS STEEL WORK","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The following in cladding","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The following in welded frame ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sundries","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["890 x 585 x 912mm High support frame for overlay sink complete (See Drawing 045-S20 attached to the back of these bills of quantities) ","No",129,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["1190 x 585 x 912mm High support frame for overlay sink (measured elsewhere)  complete (See Drawing 045-S20 attached to the back of these bills of quantities) ","No",92,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["1590 x 585 x 912mm High support frame for overlay sink (measured elsewhere)  complete (See Drawing 045-S20 attached to the back of these bills of quantities) ","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PRESSED STEEL DOOR FRAMES","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["1.2mm Double rebated frames suitable for half brick walls and fitted with one pair of screw on stainless steel ball bearing hinges per door leaf","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Frame for door 813 x 2032mm high ","No",336,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Frame for door 956 x 2032mm high ","No",24,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["1.2mm Double rebated frames suitable for one brick walls and fitted with one pair of screw on stainless steel ball bearing hinges per door leaf","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Frame for door 813 x 2032mm high ","No",26,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Frame for door 956 x 2032mm high ","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["1.2mm Purpose made frame with mitred top corners, seam welded joints and corner stiffeners in the reveals on the inside suitable for half brick walls and fitted with one pair of screw on stainless steel ball bearing hinges per door leaf","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Frame for door 505 x 1738mm high ","No",8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Frame for door 762 x 1738mm high ","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D5341*C5341","v":{"v":0,"d":"R0.00"}}]
["Frame for door 813 x 1738mm high ","No",161,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Frame for door 965 x 2032mm high ","No",680,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Frame for door 1264 x 2032mm high ","No",10,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Frame for swing door 965 x 2032mm high ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Frame for door 965 x 2032mm high with 279mm high fanlight above","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Frame for swing door 1036 x 2032mm high ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Frame for swing double door 1800 x 2032mm high ","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Frame for double door 986 x 1738mm high ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Frame for double door 1436 x 1738mm high ","No",14,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Frame for double door 1350 x 2032mm high ","No",55,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Frame for double door 1510 x 2032mm high ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Frame for double door 1800 x 2032mm high ","No",16,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["1.2mm Purpose made frame for sliding door suitable for one brick wall","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Frame for sliding door 1952 x 2100mm high ","No",11,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["1.2mm Purpose made chamfered frame for sliding door with mitred top corners, seam welded joints and corner stiffeners in the reveals on the inside suitable for half brick walls","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Frame for sliding door 952 x 2100mm high ","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Frame for sliding door 1352 x 2100mm high ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Frame for sliding door 1652 x 2100mm high ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["1.2mm Purpose made chamfered frame for sliding door with mitred top corners, seam welded joints and corner stiffeners in the reveals on the inside suitable for half brick walls","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Frame for sliding door 1952 x 2100mm high ","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["1.2mm Purpose made chamfered frame for sliding door with mitred top corners, seam welded joints and corner stiffeners in the reveals on the inside suitable for one brick walls","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Frame for sliding door 1172 x 2100mm high ","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Frame for sliding door 1352 x 2100mm high ","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Frame for sliding door 1652 x 2100mm high ","No",15,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Frame for sliding door 1952 x 2100mm high ","No",7,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Frame for double sliding door 2000 x 2032mm high ","No",19,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Frame for double sliding door 1950 x 2108mm high ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PRESSED MILD STEEL DOOR FRAMES","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["1.2mm Purpose made chamfered frame with mitred top corners, seam welded joints and corner stiffeners in the reveals on the inside suitable for one brick walls and fitted with one pair of screw on stainless steel ball bearing hinges per door leaf","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Frame for door 505 x 1738mm high ","No",15,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Frame for door 762 x 1738mm high ","No",12,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Frame for door 813 x 1738mm high ","No",57,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D5405*C5405","v":{"v":0,"d":"R0.00"}}]
["Frame for door 957 x 2032mm high ","No",15,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Frame for door 965 x 2032mm high ","No",602,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Frame for swing door 965 x 2032mm high ","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Frame for door 965 x 2032mm high with 279mm high fanlight above","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Frame for door 980 x 1565mm high ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Frame for swing door 1036 x 2032mm high ","No",45,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Frame for swing double door 1800 x 2032mm high ","No",27,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Frame for swing double door 1800 x 2032mm high with 279mm high fanlight above","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Frame for double door 1350 x 2032mm high ","No",175,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Frame for double door 1350 x 2032mm high with 279mm high fanlight above","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Frame for double door 1436 x 1738mm high ","No",51,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Frame for double door 1500 x 2032mm high ","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Frame for double door 1510 x 2032mm high ","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Frame for double door 1800 x 2032mm high ","No",108,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["STEEL STRONGROOM DOORS, VENTILATORS, ETC.","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Mutual or similar approved Strongroom doors, etc. suitable for 230mm walls fixed to brickwork or concrete","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["255 x 255mm Stainless steel double ended strongroom ventilator with drop shutter mechanism","No",18,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Mutual Austen Safes DS1 Record room door or similar approved with 1 x 7-lever security keylock finished in rustproof undercoat for final painting by contractors.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Door size 900 x 1860mm high ","No",15,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Mutual Austen Safes DS550/2 SABS Category 2 (Light Duty) Strong room door or similar approved with 2 x 7-lever security keylock finished in rustproof undercoat for final painting by contractors.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Door size 900 x 1860mm high ","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 140 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["ALUMINIUM WINDOWS, DOORS, ETC.","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: All aluminium doors, windows, shopfronts, view panels, etc. to comply with AAAMSA standards and specifications and to Architect's approval. Prices must include for the perimeters of frames to be sealed to the structure with approved sealant",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["ALUMINIUM LOUVRED VENT GRILLS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Standard colour purpose made polyester powder coated (50 - 100u) louvre vent grills and frames to doors including cutting of opening in door","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ventilation grill fitted to door size 600 x 100mm high overall ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ventilation grill fitted to door size 600 x 200mm high overall ","No",25,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ventilation grill fitted to door size 600 x 300mm high overall ","No",518,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ventilation grill fitted to door size 600 x 400mm high overall ","No",21,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ventilation grill fitted to door size 600 x 500mm high overall ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ventilation grill fitted to door size 600 x 600mm high overall ","No",182,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D5469*C5469","v":{"v":0,"d":"R0.00"}}]
["Standard colour purpose made polyester powder coated (50 - 100u) louvre vent grills and frames to brick walls including timber frame","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ventilation grill fitted to half brick wall size 400 x 600mm high overall ","No",18,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["ALUMINIUM WINDOWS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Purpose made standard colour polyester powder coated aluminium windows with glass panes and/or solid aluminium panels as stated, window furniture, screws and bolts installed complete strictly according to AAAMSA standards and specifications","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A windows as per series A-060 drawing schedules  Window Sheets: Rev01: A-060-001; A-060-002; A-060-006; A-060-008 to 012; A-060-015; A-060-017; A-060-022; A-060-024; A-060-025; A-060-026 Rev02: A-060-003 to 005; A-060-007; A-060-013; A-060-014; A-060-016; A-060-0018 to 021;  A-060-023  ","H4",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 1, size 900 x 900mm high","No",20,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 2, size 3570 x 2400mm high","No",16,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 3, size 730 x 2400mm high","No",18,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 4, size 900 x 2400mm high","No",47,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 5, size 2260 x 2400mm high","No",11,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 6, size 6801 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 7, size 5854 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 8, size 6460 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 9, size 6210 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 10, size 1880 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 11, size 1105 x 900mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 12, size 4640 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 13, size 1650 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 14, size 3868 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 15, size 2895 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 16, size 1365 x 2100mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 17, size 600 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 18, size 3330 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 19, size 3894 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 20, size 3445 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 21, size 2510 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 22, size 2030 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 23, size 2450 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 24, size 3895 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 25, size 3895 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 26, size 1500 x 1800mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 27, size 3895 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D5533*C5533","v":{"v":0,"d":"R0.00"}}]
["Block A window Type 28, size 3895 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 29, size 2782 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 30, size 2570 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 31, size 2400 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 32, size 1330 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 33, size 6820 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 34, size 4744 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 35, size 5853 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 36, size 6816 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 37, size 2260 x 1800mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 37a, size 2260 x 900mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 38, size 6816 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 39, size 5855 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 40, size 5855 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 41, size 6816 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 42, size 967 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 43, size 3000 x 1500mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 44, size 5520 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 45, size 4180 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 46, size 1555 x 2400mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 47, size 1800 x 2400mm high","No",11,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 48, size 900 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 49, size 1200 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 50, size 5250 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 51, size 2710 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 52, size 900 x 1230mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 53, size 1305 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 54, size 4970 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 55, size 2190 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 56, size 4630 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 57, size 1800 x 1500mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 58, size 1200 x 1500mm high","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D5597*C5597","v":{"v":0,"d":"R0.00"}}]
["Block A window Type 59, size 6770 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 60, size 3345 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 61, size 4520 x 2100mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 62, size 2057 x 2100mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 63, size 5860 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 64, size 4550 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 65, size 600 x 900mm high","No",9,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 66, size 3995 x 2100mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 67, size 1500 x 1500mm high","No",10,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 68, size 2460 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 69, size 4000 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 70, size 4510 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 71, size 2800 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 72, size 1370 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 73, size 2460 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 74, size 1370 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 75, size 2260 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 76, size 3055 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 77, size 6816 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 78, size 1800 x 1800mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 79, size 6800 x 2100mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 80, size 5540 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 81, size 2260 x 2400mm high","No",7,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 82, size 6825 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 83, size 1780 x 1500mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 84, size 5855 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 85, size 6795 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 86, size 5872 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 87, size 6816 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 88, size 5855 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 89, size 6460 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 90, size 6211 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D5661*C5661","v":{"v":0,"d":"R0.00"}}]
["Block A window Type 91, size 1906 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 92, size 6814 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 93, size 5855 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 94, size 5855 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 95, size 6815 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 96, size 6220 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 97, size 5855 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 98, size 5855 x 900mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 99, size 6816 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 100, size 2260 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 101, size 3895 x 1500mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 102, size 1815 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 103, size 1500 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 104, size 6800 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 105, size 3660 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 106, size 6816 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 107, size 1050 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 108, size 1120 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 109, size 2470 x 1800mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 110, size 890 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 111, size 2530 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 112, size 6850 x 1800mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 113, size 3200 x 2400mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 114, size 2520 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 115, size 3320 x 1500mm high","No",41,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 116, size 3660 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 117, size 3660 x 2100mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 118, size 730 x 2100mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 119, size 3895 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 120, size 2300 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 121, size 600 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 122, size 3415 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D5725*C5725","v":{"v":0,"d":"R0.00"}}]
["Block A window Type 123, size 2510 x 2100mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 124, size 3170 x 900mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 125, size 1650 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 126, size 3895 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 127, size 3897 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 128, size 1400 x 1500mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 129, size 3865 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 130, size 2500 x 2400mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 131, size 3858 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 132, size 3445 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 133, size 2970 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 134, size 2370 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 135, size 5895 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 136, size 3910 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 137, size 3595 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 138, size 900 x 1500mm high","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 139, size 2030 x 900mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 140, size 6420 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 141, size 4895 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 142, size 3895 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 143, size 3470 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 144, size 3895 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 145, size 2782 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 146, size 2030 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 147, size 3410 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 148, size 3900 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 149, size 2735 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 150, size 790 x 2100mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 151, size 3660 x 2100mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 152, size 3110 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 153, size 3320 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 154, size 2520 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D5789*C5789","v":{"v":0,"d":"R0.00"}}]
["Block A window Type 155, size 2840 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 156, size 2260 x 1500mm high","No",12,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 157, size 3000 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 158, size 6415 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 159, size 5854 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 160, size 6817 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 161, size 6816 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 162, size 5855 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 163, size 5855 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 164, size 6065 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 165, size 6815 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 166, size 5855 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 167, size 3845 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 168, size 6785 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 169, size 6785 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 170, size 2360 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 171, size 7250 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 172, size 4230 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 173, size 6727 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 174, size 5750 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 175, size 6800 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 176, size 2290 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 177, size 4015 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 178, size 2375 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 179, size 600 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 180, size 5650 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 181, size 7280 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 182, size 2940 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 183, size 4592 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 184, size 1400 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 185, size 1870 x 1500mm high","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 186, size 5110 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D5853*C5853","v":{"v":0,"d":"R0.00"}}]
["Block A window Type 187, size 6815 x 1200mm high","No",8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 188, size 5860 x 1200mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 189, size 6795 x 1200mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 190, size 5875 x 1200mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 191, size 4400 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 192, size 6815 x 1200mm high","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 193, size 5860 x 1200mm high","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 194, size 5860 x 1200mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 195, size 6220 x 1200mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 196, size 6815 x 1200mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 197, size 5850 x 1200mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 198, size 5855 x 1200mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 199, size 6820 x 1200mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 200, size 2450 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 201, size 3320 x 1200mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 202, size 3660 x 1200mm high","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 203, size 1700 x 1200mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 204, size 1500 x 900mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 205, size 3265 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 206, size 3890 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 207, size 3415 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 208, size 2100 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 209, size 1815 x 900mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 210, size 460 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 211, size 1855 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 212, size 600 x 900mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 213, size 1650 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 214, size 3890 x 1200mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 215, size 1500 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 216, size 3895 x 1200mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 217, size 900 x 900mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 218, size 2505 x 2400mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D5917*C5917","v":{"v":0,"d":"R0.00"}}]
["Block A window Type 219, size 3067 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 220, size 5000 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 221, size 3910 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 222, size 1200 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 223, size 1370 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 224, size 3000 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 225, size 6420 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 226, size 3895 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 227, size 2000 x 900mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 228, size 1500 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 229, size 3525 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 230, size 1110 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 231, size 3415 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 232, size 3900 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 233, size 3055 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 234, size 1700 x 1200mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 235, size 2100 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 236, size 3270 x 1200mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 237, size 3010 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 238, size 2410 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 239, size 2260 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 240, size 6815 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 241, size 5855 x 1800mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 242, size 2260 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 243, size 6820 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 244, size 5850 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 245, size 6815 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 246, size 2260 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 247, size 2265 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 248, size 6675 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 249, size 3260 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 250, size 5855 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D5981*C5981","v":{"v":0,"d":"R0.00"}}]
["Block A window Type 251, size 5855 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 252, size 6817 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 253, size 6800 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 254, size 1430 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 255, size 6210 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 256, size 2750 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 257, size 6470 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 258, size 5980 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 259, size 1055 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 260, size 7280 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 261, size 4330 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 262, size 1870 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 263, size 3550 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 264, size 7285 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 265, size 4075 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 266, size 5860 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 267, size 5110 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 268, size 1500 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 269, size 6105 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 270, size 2920 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 271, size 900 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 272, size 3920 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 273, size 460 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 274, size 5875 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 275, size 2260 x 2400mm high","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 276, size 6815 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 277, size 5855 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 278, size 1900 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 279, size 5855 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 280, size 6215 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 281, size 1000 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 282, size 6850 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D6045*C6045","v":{"v":0,"d":"R0.00"}}]
["Block A window Type 283, size 4400 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 284, size 1350 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 285, size 2260 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 286, size 2600 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 287, size 3895 x 1200mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 288, size 3415 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 289, size 1910 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 290, size 2505 x 1500mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 291, size 2895 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 292, size 3895 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 293, size 3895 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 294, size 3875 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 295, size 1800 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 296, size 2620 x 2400mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 297, size 8285 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 298, size 5860 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 299, size 4370 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 300, size 8240 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 301, size 6200 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 302, size 2505 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 303, size 1500 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 304, size 7040 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 305, size 2075 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 306, size 3895 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 307, size 3895 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 308, size 8240 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 309, size 3800 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 310, size 6270 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 311, size 5665 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 312, size 6360 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 313, size 4470 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 314, size 2780 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D6109*C6109","v":{"v":0,"d":"R0.00"}}]
["Block A window Type 315, size 3415 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 316, size 3900 x 1200mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 317, size 3055 x 1200mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 318, size 1700 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 319, size 3660 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 320, size 3660 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 321, size 3320 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 322, size 8125 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 323, size 3000 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 324, size 1817 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 325, size 6305 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 326, size 6580 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 327, size 5855 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 328, size 5840 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 329, size 6800 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 330, size 6815 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 331, size 5855 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 332, size 5855 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 333, size 6815 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 334, size 5855 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 335, size 5855 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 336, size 6815 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 337, size 2260 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 338, size 5700 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 339, size 5220 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 340, size 2060 x 2400mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 341, size 7310 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 342, size 2400 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 343, size 3930 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 344, size 2650 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 345, size 850 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 346, size 1830 x 900mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D6173*C6173","v":{"v":0,"d":"R0.00"}}]
["Block A window Type 347, size 3450 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 348, size 1900 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 349, size 5060 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 350, size 3735 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 351, size 4860 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 352, size 1680 x 1345mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 353, size 5170 x 600mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 354, size 2200 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 355, size 970 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 356, size 3000 x 1020mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 357, size 2750 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 358, size 930 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 359, size 5080 x 765mm high","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 360, size 3910 x 600mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 361, size 2500 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 362, size 3000 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 363, size 1500 x 1200mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 364, size 1200 x 1200mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 365, size 2100 x 1020mm high","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 366, size 1200 x 900mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 367, size 2000 x 600mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 368, size 722 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 369, size 1863 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 370, size 1270 x 1020mm high","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 371, size 900 x 900mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 372, size 1947 x 1025mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 373, size 2333 x 1025mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 374, size 1200 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 375, size 2600 x 900mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 376, size 1800 x 900mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 377, size 1837 x 1025mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 378, size 2120 x 1025mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D6237*C6237","v":{"v":0,"d":"R0.00"}}]
["Block A window Type 379, size 2700 x 1020mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 380, size 1158 x 1020mm high","No",8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 381, size 1046 x 1020mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 382, size 3474 x 2125mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 383, size 1030 x 1025mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 384, size 2550 x 2125mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 385, size 2580 x 1025mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 386, size 1200 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 387, size 2655 x 1025mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 388, size 1200 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 389, size 2845 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 390, size 4010 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 391, size 2805 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 392, size 1450 x 900mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 393, size 4900 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 394, size 4982 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 395, size 3143 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 396, size 1500 x 900mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 397, size 2225 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 398, size 1000 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 399, size 785 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 400, size 1000 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 401, size 722 x 1020mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 402, size 1600 x 1020mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 403, size 3000 x 1165mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 404, size 1920 x 2720mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 405, size 5804 x 17320mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 406, size 5908 x 12900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 407, size 4071 x 12240mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 408, size 14883 x 11210mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 409, size 2000 x 2000mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block A window Type 410, size 2000 x 2000mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D6301*C6301","v":{"v":0,"d":"R0.00"}}]
["Block A window Type 411, size 3000 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B windows as per series B-060 drawing schedulesWindow Sheets:Rev01:B-060-002; B-060-003; B-060-010; B-060-011; B-060-013; B-060-015Rev02: B-060-004; B-060-006; B-060-008; B-060-009; B-060-012Rev03: B-060-001; B-060-005; B-060-014","H4",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 1, size 1800 x 900mm high","No",12,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 2, size 3600 x 2100mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 3, size 1800 x 2100mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 4, size 2700 x 2100mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 5, size 900 x 1500mm high","No",36,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 6, size 900 x 900mm high","No",25,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 7, size 600 x 900mm high","No",7,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 8, size 3570 x 2100mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 9, size 1800 x 2100mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 10, size 1800 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 11, size 900 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 12, size 1800 x 1500mm high","No",41,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 13, size 1800 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 14, size 3000 x 2100mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 15, size 2400 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 16, size 5850 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 17, size 3080 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 18, size 4515 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 19, size 4492 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 20, size 600 x 900mm high","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 21, size 1500 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 22, size 600 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 23, size 900 x 2400mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 24, size 6435 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 25, size 2700 x 2400mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 26, size 3670 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 27, size 2700 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 28, size 4370 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 29, size 4153 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 30, size 960 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D6365*C6365","v":{"v":0,"d":"R0.00"}}]
["Block B window Type 31, size 6144 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 32, size 900 x 2100mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 33, size 2610 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 34, size 4210 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 35, size 2200 x 900mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 36, size 1800 x 900mm high","No",10,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 37, size 1910 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 38, size 4153 x 2400mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 39, size 3450 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 40, size 5370 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 41, size 4850 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 42, size 1410 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 43, size 840 x 1800mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 44, size 2900 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 45, size 900 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 46, size 1800 x 2400mm high","No",9,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 47, size 1079 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 48, size 1281 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 49, size 2400 x 1500mm high","No",7,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 50, size 900 x 900mm high","No",38,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 51, size 3570 x 1500mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 52, size 3170 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 53, size 6300 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 54, size 750 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 55, size 3180 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 56, size 2700 x 1800mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 57, size 1800 x 1800mm high","No",27,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 58, size 7380 x 2400mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 59, size 2790 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 60, size 6100 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 61, size 3995 x 2400mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 62, size 2530 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D6429*C6429","v":{"v":0,"d":"R0.00"}}]
["Block B window Type 63, size 1760 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 64, size 970 x 1500mm high","No",8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 65, size 2100 x 1500mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 66, size 1200 x 1500mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 67, size 2280 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 68, size 2700 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 69, size 2640 x 2400mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 70, size 3560 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 71, size 2640 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 72, size 6060 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 73, size 5340 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 74, size 2970 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 75, size 5360 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 76, size 5160 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 77, size 4330 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 78, size 2595 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 79, size 1500 x 1500mm high","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 80, size 730 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 81, size 900 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 82, size 2700 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 83, size 1280 x 1500mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 84, size 2400 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 85, size 1014 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 86, size 2400 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 87, size 2000 x 1500mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 88, size 1500 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 89, size 665 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 90, size 1120 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 91, size 1450 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 91, size 1450 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 92, size 1240 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 93, size 790 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D6493*C6493","v":{"v":0,"d":"R0.00"}}]
["Block B window Type 94, size 2750 x 1800mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 95, size 2400 x 1500mm high","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 96, size 2750 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 97, size 900 x 1800mm high","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 98, size 1660 x 1800mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 99, size 2700 x 1800mm high","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 100, size 3400 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 101, size 1605 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 102, size 1800 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 103, size 900 x 1800mm high","No",11,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 104, size 2157 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 105, size 750 x 1800mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 106, size 2260 x 1800mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 107, size 1020 x 1800mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 108, size 2280 x 1800mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 109, size 1800 x 2400mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 110, size 860 x 900mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 111, size 1410 x 1800mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 112, size 2700 x 1800mm high","No",8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 113, size 2700 x 1500mm high","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 114, size 2370 x 1800mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 115, size 4940 x 2400mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 116, size 3770 x 1800mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 117, size 1300 x 1800mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 118, size 1520 x 1800mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 119, size 1590 x 900mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 120, size 3400 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 121, size 1850 x 900mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 122, size 2700 x 2400mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 123, size 6060 x 2400mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 124, size 1400 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 125, size 2400 x 1800mm high","No",10,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D6557*C6557","v":{"v":0,"d":"R0.00"}}]
["Block B window Type 126, size 6720 x 2400mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 127, size 1540 x 2400mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 128, size 1200 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 129, size 2580 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 130, size 2910 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 131, size 2200 x 1800mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 132, size 3915 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 133, size 4745 x 1800mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 134, size 4860 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 135, size 1710 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 136, size 700 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 137, size 1630 x 900mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 138, size 3570 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 139, size 820 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 140, size 5170 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 141, size 4175 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 142, size 3920 x 1800mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 143, size 4485 x 1800mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 144, size 4430 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 145, size 3370 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 146, size 1585 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 147, size 2500 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 148, size 2640 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 149, size 1500 x 1020mm high","No",69,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 150, size 2960 x 1020mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 151, size 900 x 1020mm high","No",14,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 152, size 1800 x 1020mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 153, size 2910 x 2465mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 154, size 1500 x 2465mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 155, size 3320 x 2465mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 156, size 3278 x 2465mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 157, size 4720 x 2465mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D6621*C6621","v":{"v":0,"d":"R0.00"}}]
["Block B window Type 158, size 1300 x 2725mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 159, size 1690 x 2725mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 160, size 2360 x 2725mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 161, size 6451 x 2725mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 162, size 3713 x 2725mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 163, size 5841 x 2725mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 164, size 6693 x 2725mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 165, size 5633 x 2725mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 166, size 5413 x 2725mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 167, size 653 x 2725mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 168, size 600 x 1020mm high","No",7,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 169, size 2910 x 2465mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 170, size 2350 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 171, size 3594 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 172, size 1500 x 3060mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 173, size 3320 x 3060mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 174, size 4720 x 3060mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 175, size 3278 x 3060mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 176, size 1300 x 4120mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 177, size 6451 x 4120mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 178, size 2360 x 4120mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 179, size 6451 x 4120mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 180, size 3713 x 4120mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 181, size 5841 x 4120mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 182, size 6693 x 4120mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 183, size 5633 x 4120mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 184, size 653 x 4120mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 185, size 650 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 186, size 1650 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 187, size 1250 x 1020mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 188, size 2600 x 1020mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 189, size 2510 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D6685*C6685","v":{"v":0,"d":"R0.00"}}]
["Block B window Type 190, size 832 x 1020mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 191, size 6145 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 192, size 2843 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 193, size 2940 x 1020mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 194, size 2740 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 195, size 1478 x 1195mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 196, size 6693 x 3260mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 197, size 5633 x 3260mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 198, size 1238 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 199, size 1692 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 200, size 2100 x 1020mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 201, size 1200 x 1020mm high","No",17,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 202 size 2400 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 203, size 2325 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 204, size 765 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 205, size 1403 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 206, size 667 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 207, size 1400 x 1195mm high","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 208, size 1615 x 1195mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 209, size 2077 x 1195mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 210, size 3180 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 211, size 920 x 1025mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 212, size 3510 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 213, size 2200 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 214, size 3377 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 215, size 2120 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 216, size 3893 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 217, size 1305 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 218, size 2388 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 219, size 1713 x 1020mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 220, size 3472 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 221, size 3983 x 1020mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D6749*C6749","v":{"v":0,"d":"R0.00"}}]
["Block B window Type 222, size 1500 x 2125mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 223, size 3320 x 2125mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 224, size 3278 x 2125mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 225, size 4720 x 2125mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 226, size 1300 x 2920mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 227, size 1690 x 2920mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 228, size 2360 x 2920mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 229, size 6451 x 2920mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 230, size 3713 x 2920mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 231, size 5841 x 2920mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 232, size 2400 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 233, size 1500 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 234, size 2600 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 235, size 3970 x 900mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 236, size 3840 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 237, size 3000 x 900mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 238, size 3685 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 239, size 1800 x 900mm high","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 240, size 3000 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 241, size 6100 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 242, size 1800 x 1200mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 243, size 809 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 244, size 720 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 245, size 3500 x 900mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 246, size 4997 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 247, size 3227 x 1800mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 248, size 5830 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 249, size 3155 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 250, size 7500 x 2125mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 251, size 700 x 3260mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 252, size 2000 x 1530mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 253, size 1800 x 1530mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D6813*C6813","v":{"v":0,"d":"R0.00"}}]
["Block B window Type 254, size 928 x 1530mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 255, size 7276 x 3275mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 256, size 700 x 2720mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 257, size 4500 x 1975mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 258, size 12 354 x 17 135mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 259, size 12 435 x 17 135mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 260, size 1400 x 1400mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 261, size 15 480 x 9158mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block B window Type 262, size 8785 x 1485mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C windows as per series C-060 drawing schedules  Window Sheets: Rev01: C-060-001 to 010; C-060-012 to 014 Rev02: C-060-011","H4",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 1, size 800 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 2, size 1800 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 3, size 2000 x 1500mm high","No",12,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 4, size 2970 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 5, size 2000 x 900mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 6, size 2780 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 7, size 3220 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 8, size 1630 x 2100mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 9, size 1450 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 10, size 1400 x 2100mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 11, size 2400 x 2100mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 12, size 1800 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 13, size 1500 x 900mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 14, size 1500 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 15, size 2588 x 2100mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 16, size 2670 x 2100mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 17, size 900 x 2100mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 18, size 2525 x 2100mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 19, size 3095 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 20, size 3380 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 21, size 6710 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 22, size 2880 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D6877*C6877","v":{"v":0,"d":"R0.00"}}]
["Block C window Type 23, size 600 x 900mm high","No",17,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 24, size 900 x 900mm high","No",20,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 25, size 1540 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 26, size 6765 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 27, size 3000 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 28, size 1580 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 29, size 3699 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 30, size 1450 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 31, size 1110 x 1500mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 32, size 1800 x 1500mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 33, size 3820 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 34, size 3720 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 35, size 1200 x 1200mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 36, size 900 x 900mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 37, size 2400 x 1500mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 38, size 2100 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 39, size 2100 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 40, size 2260 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 41, size 2670 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 42, size 3220 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 43, size 1210 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 44, size 870 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 45, size 1800 x 1500mm high","No",16,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 46, size 1500 x 900mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 47, size 900 x 1200mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 48, size 3000 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 49, size 1500 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 50, size 3000 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 51, size 3000 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 52, size 1475 x 2700mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 53, size 1475 x 2700mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 54, size 3970 x 2700mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D6941*C6941","v":{"v":0,"d":"R0.00"}}]
["Block C window Type 55, size 2100 x 1200mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 56, size 4470 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 57, size 4610 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 58, size 900 x 1200mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 59, size 2100 x 900mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 60, size 1500 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 61, size 1500 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 62, size 1200 x 1500mm high","No",7,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 63, size 4000 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 64, size 4000 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 65, size 5000 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 66, size 1760 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 67, size 1310 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 68, size 3300 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 69, size 2280 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 70, size 4000 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 71, size 1200 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 72, size 1200 x 1200mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 73, size 2055 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 74, size 3790 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 75, size 3970 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 76, size 1102 x 2400mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 77, size 2400 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 78, size 1800 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 79, size 1500 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 80, size 1500 x 1800mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 81, size 2400 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 82, size 4000 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 83, size 4173 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 84, size 5860 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 85, size 1270 x 2700mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 86, size 1460 x 2700mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D7005*C7005","v":{"v":0,"d":"R0.00"}}]
["Block C window Type 87, size 1500 x 1500mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 88, size 1500 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 89, size 1800 x 1200mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 90, size 3000 x 1200mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 91, size 5740 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 92, size 2000 x 1500mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 93, size 6830 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 94, size 2370 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 95, size 1500 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 96, size 3300 x 1200mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 97, size 4340 x 1200mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 98, size 2400 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 99, size 2650 x 1200mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 100, size 2200 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 101, size 2460 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 102, size 1000 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 103, size 2110 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 104, size 3130 x 1200mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 105, size 3220 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 106, size 1500 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 107, size 4000 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 108, size 900 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 109, size 1500 x 2400mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 110, size 2400 x 1500mm high","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 111, size 600 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 112, size 4055 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 113, size 2530 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 114, size 3600 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 115, size 7169 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 116, size 5779 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 117, size 1200 x 900mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 118, size 5775 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D7069*C7069","v":{"v":0,"d":"R0.00"}}]
["Block C window Type 119, size 1800 x 2400mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 120, size 1800 x 1200mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 121, size 4670 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 122, size 2000 x 1500mm high","No",19,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 123, size 2310 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 124, size 2817 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 125, size 3200 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 126, size 2742 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 127, size 2100 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 128, size 1180 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 129, size 7340 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 130, size 1580 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 131, size 2480 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 132, size 1953 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 133, size 2400 x 1200mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 134, size 1200 x 1200mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 135, size 2970 x 1200mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 136, size 3735 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 137, size 1740 x 1200mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 138, size 2100 x 1200mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 139, size 4440 x 1200mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 140, size 3042 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 141, size 1660 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 142, size 815 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 143, size 2400 x 1500mm high","No",7,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 144, size 1500 x 1200mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 145, size 1800 x 900mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 146, size 3570 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 147, size 2400 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 148, size 1800 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 149, size 2400 x 1200mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 150, size 2970 x 1200mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D7133*C7133","v":{"v":0,"d":"R0.00"}}]
["Block C window Type 151, size 3720 x 1200mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 152, size 2846 x 1200mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 153, size 1030 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 154, size 6709 x 600mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 155, size 1904 x 600mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 156, size 6570 x 1200mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 157, size 3490 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 158, size 900 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 159, size 4540 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 160, size 6798 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 161, size 5774 x 1200mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 162, size 3500 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 163, size 1200 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 164, size 2845 x 1500mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 165, size 2400 x 1200mm high","No",10,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 167, size 1940 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 168, size 4190 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 169, size 5050 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 170, size 3000 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 171, size 780 x 1200mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 172, size 2840 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 173, size 1800 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 174, size 15500 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 175, size 11080 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 176, size 1200 x 900mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 177, size 3890 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 178, size 6700 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 179, size 1400 x 2700mm high","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 180, size 3550 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 181, size 2582 x 600mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 182, size 6802 x 600mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 183, size 3600 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D7197*C7197","v":{"v":0,"d":"R0.00"}}]
["Block C window Type 184, size 1800 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 184a, size 2400 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 185, size 900 x 1048mm high","No",16,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 186, size 1220 x 1270mm high","No",10,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 187, size 1902 x 1270mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 188, size 2107 x 1270mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 189, size 2600 x 1345mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 190, size 370 x 1245mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 191, size 1455 x 1245mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 192, size 900 x 1360mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 193, size 4125 x 1360mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 194, size 1573 x 1360mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 195, size 973 x 1360mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 196, size 2534 x 1360mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 197, size 1670 x 1020mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 199, size 2600 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 200, size 900 x 1020mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 201, size 3000 x 1025mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 202, size 3650 x 1325mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 203, size 1200 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 204, size 4000 x 600mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 205, size 1200 x 600mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 206, size 1500 x 600mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 207, size 3000 x 1020mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 208, size 700 x 595mm high","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 209, size 1500 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 210, size 808 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 211, size 2627 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 212, size 3093 x 1020mm high","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 213, size 11390 x 680mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 214, size 5720 x 680mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 215, size 7220 x 685mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D7261*C7261","v":{"v":0,"d":"R0.00"}}]
["Block C window Type 216, size 1865 x 685mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 217, size 6300 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 218, size 4460 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 219, size 3040 x 1190mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 220, size 4980 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 221, size 6900 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 222, size 2159 x 1190mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 223, size 693 x 1190mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 224, size 2400 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 225, size 1668 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 226, size 2927 x 1870mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 227, size 4553 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 228, size 900 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 229, size 4200 x 1020mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 230, size 3000 x 600mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 231, size 773 x 1020mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 232, size 1773 x 1020mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 233, size 1173 x 1020mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 234, size 1987 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 235, size 1912 x 1025mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 236, size 1800 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 237, size 1400 x 600mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 238, size 1800 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 239, size 498 x 2125mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 240, size 4495 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 241, size 3950 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 242, size 2430 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 243, size 1500 x 1205mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block C window Type 244, size 2700 x 1205mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D windows as per  D-060 drawing schedulesWindow Sheets:Rev01: D-060-001; D-060-004 to 007: D-060-015; D-060-016Rev02:D-060-002; D-060-003; D-060-008; D-060-010 to 013; D-060-017Rev03:D-060-009; D-060-014","H4",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 1, size 5790 x 2100mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 2, size 1660 x 2100mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D7325*C7325","v":{"v":0,"d":"R0.00"}}]
["Block D window Type 3, size 900 x 900mm high","No",7,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 4, size 5315 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 5, size 3480 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 6, size 2400 x 900mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 7, size 5400 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 8, size 4285 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 9, size 2700 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 10, size 4050 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 11, size 1800 x 900mm high","No",7,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 12, size 5645 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 13, size 5450 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 14, size 1500 x 1800mm high","No",7,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 15, size 3235 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 16, size 1800 x 900mm high","No",11,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 17, size 2200 x 1800mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 18, size 7100 x 2100mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 19, size 1500 x 900mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 20, size 1800 x 900mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 21, size 4180 x 900mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 22, size 1800 x 1500mm high","No",15,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 23, size 5400 x 1500mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 24, size 4300 x 1500mm high","No",13,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 25, size 3700 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 26, size 3170 x 1500mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 27, size 4250 x 1500mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 28, size 3165 x 1500mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 29, size 5810 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 30, size 3950 x 900mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 31, size 7130 x 900mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 32, size 5810 x 1200mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 33, size 1800 x 2100mm high","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 34, size 3010 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D7389*C7389","v":{"v":0,"d":"R0.00"}}]
["Block D window Type 35, size 2650 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 36, size 2740 x 1500mm high","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 37, size 1600 x 2100mm high","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 38, size 900 x 2100mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 39, size 2100 x 2100mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 40, size 2100 x 900mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 41, size 5540 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 42, size 2500 x 1800mm high","No",8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 43, size 2000 x 900mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 44, size 2300 x 1500mm high","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 45, size 2000 x 1500mm high","No",7,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 46, size 530 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 47, size 1420 x 1500mm high","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 48, size 3480 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 49, size 3000 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 50, size 2335 x 1500mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 51, size 900 x 900mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 52, size 4000 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 53, size 7580 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 54, size 1470 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 55, size 2700 x 1800mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 56, size 3000 x 1500mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 57, size 1500 x 900mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 58, size 2042 x 1200mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 59, size 4960 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 60, size 5330 x 2100mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 61, size 2800 x 2400mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 62, size 1800 x 2400mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 63, size 3910 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 64, size 7400 x 1500mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 65, size 5780 x 1500mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 66, size 4200 x 1500mm high","No",8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D7453*C7453","v":{"v":0,"d":"R0.00"}}]
["Block D window Type 67, size 7350 x 1500mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 68, size 7080 x 1500mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 69, size 5765 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 70, size 4275 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 71, size 5780 x 1800mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 72, size 2740 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 73, size 3260 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 74, size 1260 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 75, size 1260 x 1500mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 76, size 1265 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 77, size 6240 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 78, size 1980 x 1800mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 79, size 1100 x 1800mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 80, size 1990 x 1800mm high","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 81, size 1320 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 82, size 3120 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 83, size 1550 x 2400mm high","No",8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 84, size 1505 x 1800mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 85, size 2730 x 2100mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 86, size 3055 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 87, size 5251 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 88, size 5000 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 89, size 2240 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 90, size 6420 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 91, size 5910 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 92, size 1000 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 93, size 5860 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 94, size 6380 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 95, size 5560 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 96, size 5122 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 97, size 5822 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 98, size 6274 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D7517*C7517","v":{"v":0,"d":"R0.00"}}]
["Block D window Type 99, size 4920 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 100, size 2780 x 2400mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 101, size 3040 x 1800mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 102, size 6160 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 103, size 3975 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 104, size 2400 x 1800mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 105, size 4945 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 106, size 4540 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 107, size 2330 x 900mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 108, size 2790 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 109, size 5780 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 110, size 3820 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 111, size 4300 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 112, size 1325 x 900mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 113, size 2370 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 114, size 3955 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 115, size 1995 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 116, size 2170 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 117, size 5520 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 118, size 3820 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 119, size 7000 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 120, size 3675 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 121, size 900 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 122, size 5790 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 123, size 1640 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 124, size 2400 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 125, size 4300 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 126, size 3170 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 127, size 5050 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 128, size 1390 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 129, size 2360 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 130, size 5875 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D7581*C7581","v":{"v":0,"d":"R0.00"}}]
["Block D window Type 131, size 2615 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 132, size 1350 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 133, size 1790 x 1800mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 134, size 3295 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 135, size 5550 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 136, size 4300 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 137, size 4480 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 138, size 1800 x 900mm high","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 139, size 1630 x 900mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 140, size 7100 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 141, size 3970 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 142, size 2895 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 143, size 3100 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 144, size 3560 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 145, size 1805 x 900mm high","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 146, size 4045 x 1800mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 147, size 4190 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 148, size 3170 x 2100mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 149, size 1445 x 2100mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 150, size 1800 x 900mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 151, size 1445 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 152, size 900 x 900mm high","No",10,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 153, size 690 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 154, size 4080 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 155, size 630 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 156, size 3200 x 1800mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 157, size 2965 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 158, size 1770 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 159, size 5000 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 160, size 6340 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 161, size 6520 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 162, size 2500 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D7645*C7645","v":{"v":0,"d":"R0.00"}}]
["Block D window Type 163, size 1500 x 1500mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 164, size 3060 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 165, size 5920 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 166, size 3185 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 167, size 3630 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 168, size 6665 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 169, size 3040 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 170, size 3520 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 171, size 2740 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 172, size 3260 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 173, size 1260 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 174, size 2730 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 175, size 900 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 176, size 5920 x 2400mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 177, size 7100 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 178, size 1380 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 179, size 5440 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 180, size 1740 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 181, size 4430 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 182, size 5251 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 183, size 5910 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 184, size 1440 x 1500mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 185, size 2240 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 186, size 6420 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 187, size 7390 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 188, size 4430 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 189, size 5122 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 190, size 5822 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 191, size 3105 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 192, size 6160 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 193, size 6090 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 194, size 4540 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D7709*C7709","v":{"v":0,"d":"R0.00"}}]
["Block D window Type 195, size 7400 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 196, size 3220 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 197, size 3820 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 198, size 7400 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 199, size 4195 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 200, size 4710 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 201, size 3420 x 1800mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 202, size 1050 x 1800mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 203, size 900 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 204, size 3665 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 205, size 2475 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 206, size 7340 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 207, size 7580 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 208, size 7580 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 209, size 6555 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 210, size 3095 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 211, size 2205 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 212, size 3910 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 213, size 4895 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 214, size 830 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 215, size 5445 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 216, size 3275 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 217, size 2470 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 218, size 4746 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 219, size 4710 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 220, size 1800 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 221, size 653 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 222, size 1833 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 223, size 1500 x 1020mm high","No",44,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 224, size 900 x 1020mm high","No",10,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 225, size 2000 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 226, size 6380 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D7773*C7773","v":{"v":0,"d":"R0.00"}}]
["Block D window Type 227, size 2400 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 228, size 2288 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 229, size 898 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 230, size 3035 x 1020mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 231, size 1363 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 232, size 1000 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 233, size 3893 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 234, size 2700 x 2125mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 235, size 4500 x 2125mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 236, size 4735 x 2125mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 237, size 868 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 238, size 860 x 2125mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 239, size 2790 x 2125mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 240, size 1690 x 2125mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 241, size 1810 x 2125mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 242, size 1323 x 2125mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 243, size 2412 x 2125mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 244, size 1965 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 245, size 1305 x 1020mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 246, size 2632 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 247, size 2547 x 1020mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 248, size 1200 x 1020mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 249, size 2170 x 2125mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 250, size 2600 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 251, size 2665 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 252, size 2873 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 253, size 8573 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 254, size 1720 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 255, size 9500 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 256, size 3183 x 1020mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 257, size 2240 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 258, size 2455 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D7837*C7837","v":{"v":0,"d":"R0.00"}}]
["Block D window Type 259, size 2671 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 260, size 3025 x 1020mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 261, size 8448 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 262, size 1760 x 2100mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 263, size 1380 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 264, size 1290 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 265, size 4200 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 266, size 4200 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 267, size 3520 x 2100mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 268, size 4090 x 2100mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 269, size 2400 x 900mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 270, size 5000 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 271, size 2440 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 272, size 6020 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 273, size 2000 x 1530mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 274, size 1800 x 1530mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 275, size 3500 x 16320mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 276, size 7680 x 9164mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 277, size 4500 x 1975mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block D window Type 278, size 1400 x 1400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block E windows as per series E-060 drawing schedules  Window Sheets: Rev01: E-060-001 to 002","H4",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block E window Type 1, size 4200 x 1500mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block E window Type 2, size 2000 x 1500mm high","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block E window Type 3, size 2000 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block E window Type 4, size 1200 x 2100mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block E window Type 5, size 3000 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block E window Type 6, size 600 x 900mm high","No",8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block E window Type 7, size 1500 x 900mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block E window Type 8, size 1800 x 1500mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block E window Type 9, size 2400 x 1200mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block E window Type 10, size 4200 x 1200mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block E window Type 11, size 1800 x 1200mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D7901*C7901","v":{"v":0,"d":"R0.00"}}]
["Block E window Type 12, size 3000 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block E window Type 13, size 1500 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block E window Type 14, size 4000 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block E window Type 15, size 1500 x 1200mm high","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block E window Type 16, size 3610 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block E window Type 17, size 900 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block E window Type 18, size 1800 x 900mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block E window Type 19, size 4170 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block E window Type 20, size 2400 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block E window Type 21, size 1760 x 1200mm high","No",8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block E window Type 22, size 3480 x 1200mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block E window Type 23, size 1760 x 1200mm high","No",12,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block E window Type 24, size 2300 x 905mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block E window Type 25, size 3250 x 905mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block E window Type 26, size 1160 x 905mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block E window Type 27, size 4642 x 1245mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block E window Type 28, size 4585 x 1245mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block E window Type 29, size 1718 x 1245mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block E window Type 30, size 2000 x 1245mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block E window Type 31, size 2425 x 1245mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block E window Type 32, size 803 x 1245mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block E window Type 33, size 2522 x 1245mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block E window Type 34, size 1500 x 1245mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block E window Type 35, size 2873 x 1245mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block E window Type 36, size 3208 x 1245mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block E window Type 37, size 1563 x 1245mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block E window Type 38, size 3595 x 1245mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block E window Type 39, size 2945 x 1245mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F windows as per series F-060 drawing schedulesWindow Sheets:Rev01: F-060-001 ; F-060-003Rev03:F-060-002","H4",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 1, size 1992 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 2, size 8612 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 3, size 1435 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D7965*C7965","v":{"v":0,"d":"R0.00"}}]
["Block F window Type 4, size 6465 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 5, size 900 x 900mm high","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 6, size 1840 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 7, size 1910 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 8, size 1500 x 900mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 9, size 6420 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 10, size 6340 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 11, size 3282 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 12, size 2898 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 13, size 6400 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 14, size 1800 x 900mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 15, size 1500 x 900mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 16, size 1200 x 1500mm high","No",13,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 17, size 900 x 1500mm high","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 18, size 1800 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 19, size 3800 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 20, size 900 x 1500mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 21, size 600 x 900mm high","No",10,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 22, size 1800 x 1500mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 23, size 1800 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 24, size 4170 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 25, size 1800 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 26, size 600 x 1500mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 27, size 1800 x 900mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 28, size 1800 x 2400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 29, size 1200 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 30, size 600 x 2100mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 31, size 1800 x 2100mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 32, size 3570 x 2100mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 33, size 2400 x 1500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 34, size 1800 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 35, size 1800 x 1800mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D8029*C8029","v":{"v":0,"d":"R0.00"}}]
["Block F window Type 36, size 3570 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 37, size 3378 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 38, size 943 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 39, size 2400 x 1020mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 40, size 1150 x 1750mm high","No",10,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 40a, size 4297 x 2635mm high","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 41, size 1000 x 1530mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 42, size 615 x 1785mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 43, size 2637 x 1785mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 44, size 3047 x 1785mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 45, size 4188 x 1785mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 46, size 5867 x 1785mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 47, size 4039 x 1785mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 48, size 5904 x 1785mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 49, size 1800 x 1785mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 50, size 2500 x 2500mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 51, size 1800 x 3600mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 52, size 2000 x 2000mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block F window Type 53, size 3000 x 3000mm high","No",7,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block G windows as per series G-060 drawing schedulesWindow Sheets:Rev00: G-060-001 to 002","H4",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block G window Type 01, size 1800 x 1800mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block G window Type 02, size 1696 x 1800mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block G window Type 03, size 3220 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block G window Type 04, size 440 x 1800mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block G window Type 05, size 700 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block G window Type 06, size 500 x 1800mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block G window Type 07, size 3500 x 1800mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block G window Type 08, size 1090 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block G window Type 09, size 5626 x 1800mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block G window Type 10, size 600 x 2100mm high","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block G window Type 11, size 7288 x 1800mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block G window Type 12, size 1400 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D8093*C8093","v":{"v":0,"d":"R0.00"}}]
["Block G window Type 13, size 900 x 1500mm high","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block G window Type 14, size 4000 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block G window Type 15, size 600 x 900mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block G window Type 16, size 2500 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block G window Type 17, size 1700 x 1800mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block G window Type 18, size 3270 x 1800mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block G window Type 19, size 900 x 1500mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block G window Type 20, size 2000 x 900mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block G window Type 21, size 1500 x 900mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block G window Type 22, size 3240 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block G window Type 23, size 3845 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block G window Type 24, size 3000 x 900mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block G window Type 25, size 900 x 1200mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block G window Type 26, size 2000 x 1200mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Block G window Type 27, size 2455 x 2295mm high","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sundries","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["2 x 3mm Thick aluminium plates, each 85mm wide fixed to aluminium window or door frame on one side and soft joints with approved sealant against plastered or tiled wall on other side (Typ-043-052)","m",619,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SHOWER DOORS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Powder coated aluminium shower cubicle panel and doors complete with magnetic door catch, handles, handle edge rail, receiving wall rail, hinges, etc. and toughened  safety glass, complying with SANS 1263 Part 1, 2 or 3 with name of manufacturer permanently marked on each sheet visible after glazing, in accordance with NBR N schedule 1 and SANS 10137:2002. Plugged to tiled walls including pointing all round both sides of frame (San041/041A, San077/077a)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Purpose made Shower cubicle doors overall size 900 x 2000mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Purpose made Shower cubicle doors and panel overall size 910 x 2000mm high (Door size 730 x 2000mm high)","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Purpose made Shower cubicle doors and panel overall size 1110 x 2000mm high (Door size 730 x 2000mm high)","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Purpose made Shower cubicle doors and panel overall size 1210 x 2000mm high (Door size 730 x 2000mm high)","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Purpose made Shower cubicle doors and panel corner unit overall size 1900 x 2000mm high (Door size 730 x 2000mm high)","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["GALVANISED IBR WALL PANEL","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["0.58mm IBR light industrial galvanised sheet steel with Chromadek finish (colour to Architect's approval) to one side, in single lengths fixed to external face of fire rated drywall partition (drywall partition measured elsewhere) or similar approved. All in accordance with the manufacturer's instructions, including all necessary sealer strips on overlaps, etc.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Vertical cladding","m2",353,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SUN LOUVRE SYSTEM","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Hunter Douglas No.132 sun louvre system or similar approved, colour (to be confirmed) louvre units fixed to brickwork or concrete","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sun louvre system","m2",129,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Hunter Douglas 84R vertical fixed system comprising 0,6mm thick 84R panels at 74mm centres with 60μm Luxacote® or similar approved, finish colour - to Architect’s approval, fixed to steel structure of building (measured elsewhere) using stringer and rectangular hollow section. The whole to be designed and installed by approved specialist, all in accordance with the manufacturer`s recommendations. (See Drawing G1-014-001 & G3-014-003 attached to the back of these bills of quantities)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sun louvre fixed to steel beam","m2",19,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D8157*C8157","v":{"v":0,"d":"R0.00"}}]
["FRAMELESS SHOPFRONTS AND LOBBY SCREENS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["8mm Frameless solar E-gray plus armour plate toughened safety glass fixed to steel frame with approved stainless steel spider brackets (See Drawing B-042-002 & D-042-002 attached to the back of these bills of quantities)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Glazing fixed to steel canopy (elsewhere measured) ","m2",601,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TOTAL METALWORK",null,0,null,{"$f":"SUM(E5085:E8163)","v":{"v":0,"d":"0.00"}}]
[null,null,0,null,{"v":0,"d":"R0.00"}]
["SECTION 2","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NEW HOSPITAL ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["BILL NO 12","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PLASTERING","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PREAMBLES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Preambles for Trades as defined in Scope of Work (C3.1 Item 4.1 & Item 4.2)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TRADE NAMES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Any reference to trade names in the Bills of Quantities or  Architect's specification or drawings shall deem to mean \"or similar and approved\"",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 142 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["GRANOLITHIC","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Untinted granolithic on concrete ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["32mm Thick on floors with steel trowelled finish","m2",1592,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["32mm Thick on floors with wood trowelled finish","m2",193,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["75mm High coved skirting ","m",2508,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SCREEDS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["1:3 Cement plaster screeds on concrete","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["30mm Thick on floors","m2",79879,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["30mm Thick on treads and risers of stairs","m2",952,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Average 80mm Thick on concrete roofs to falls and currents ","m2",13190,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["50mm Triangular fillet ","m",7473,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but circular on plan","m",63,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Brush finished untinted cement floor screeds on concrete composed of 1 part Cemcrete Colorcem or equally approved and 4 parts sand","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["25mm Thick on floors with brush finish","m2",546,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SPECIALIST FLOOR COVERINGS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["3mm Thick \"Levelite\" or similar approved self-levelling screeds (approved and installed by flooring sub-contractor) on concrete surface beds to obtain a level surface and providing a quality base. Sub surface to be primed and dry (moisture test to be done) to ensure a quality and sound application,  all applied in strict accordance with the manufacturer's specifications, on: ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On floors ","m2",62915,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["4mm Thick Polyurethane cement is a multi-component, medium to high strength coloured polyurethane modified, cement and aggregate screed with self-smoothing properties. It has an aesthetic, easy to clean, smooth textured aggregate surface providing medium slip resistance strictly in accordance with the manufacturer's specifications (A76)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On floors ","m2",8345,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D8221*C8221","v":{"v":0,"d":"R0.00"}}]
["200mm High coved skirting","m",3204,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["6mm Polyurethane screed with a multi-component , resin rich, smooth trowel grade, coloured polyurethane modified, cement and aggregate screed suitable for floors subject to heavy loading, abrasion and chemical exposure. It has a textured aggregate surface providing medium to heavy profile slip resistance and is typically installed at 6mm thick. The substrate and uncured floor must be at least 3°C above dew point to reduce the risk of condensation or blooming on the floor finish. Application to be strictly in accordance with manufacturer's specifications (A8)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On floors ","m2",2793,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["200mm High coved skirting","m",1603,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Prepare the concrete sub-base by mechanical grinning washing all in accordance with the manufacturer's technical specification. Prime with one coat of Sikafloor®-161 then a scratch coat of SikaFloor-161, apply base coat Sikafloor®-263 SL and broadcast to excess with Sika Deco Filler. System seal with one coat Sikafloor®-66 ZA or similar approved. All to manufacturer’s detail specifications (A77)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On floors ","m2",370,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["200mm High coved skirting","m",405,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["INTERNAL PLASTER","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["One coat 1:4 cement plaster on concrete with steel trowel ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On soffits of concrete slabs","m2",1133,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On raking soffits of ramps and stairs","m2",658,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["One coat 1:4 cement plaster on concrete with steel trowel and no other finish (Ref. C1) ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On walls","m2",2354,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["One coat 1:6 cement plaster on brickwork with wood trowel to receive wall tiling (Ref. C2 & C34)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On walls","m2",9657,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On narrow widths","m2",202,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["One coat 1:6 cement plaster on partitions with wood trowel to receive wall tiling (Ref. C2 & C34)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On walls","m2",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["One coat 1:6 cement plaster on brickwork with steel trowel (Ref. C5) ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On walls","m2",29251,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On  circular walls","m2",224,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On narrow widths","m2",1463,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["One coat 1:4 cement plaster on concrete with steel trowel (Ref. C5) ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On walls","m2",6801,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On narrow widths","m2",128,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Two coats plaster with 1:6 cement plaster finished with skim finishing coat on brickwork with steel trowel (Ref. C3)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On walls","m2",107490,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On circular walls","m2",108,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On narrow widths","m2",2943,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Two coats plaster with 1:4 cement plaster finished with skim finishing coat on concrete with steel trowel (Ref. C3)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On walls","m2",17860,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On circular columns","m2",239,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D8285*C8285","v":{"v":0,"d":"R0.00"}}]
["EXTERNAL PLASTER","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["One coat 1:4 cement plaster on concrete with woo trowel ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On soffits of concrete slabs","m2",7891,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On raking soffits of ramps and stairs","m2",1401,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["One coat 1:6 cement plaster on brickwork with steel trowel (Ref. C5) ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On walls","m2",3598,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On narrow widths","m2",129,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["One coat 1:4 cement plaster on concrete with steel trowel (Ref. C5) ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On walls","m2",1778,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On narrow widths","m2",36,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On external sills sloping not exceeding 300mm wide or high including polyurethane sealant.","m",28,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["One coat 1:6 cement plaster on brickwork with wood trowel (Ref. H14, H38, H65, H230, H239 & H277)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On walls","m2",50342,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On circular walls","m2",326,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On narrow widths","m2",2452,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On external sills sloping not exceeding 300mm wide or high including polyurethane sealant.","m",5809,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On external parapet walls sloping not exceeding 300mm wide or high all as per detail drawing HDG TYPE-042-010","m",54,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["One coat 1:4 cement plaster on concrete with wood trowel (Ref. H14, H38, H65, H230, H239 & H277)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On columns","m2",3557,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On Walls","m2",9692,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On circular walls","m2",142,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On narrow widths","m2",214,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On beams","m2",26878,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On circular upstand beams","m2",269,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["CORNER PROTECTORS, DIVIDING STRIPS, NOSING STRIPS ETC.","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["25mm x 3mm Brass dividing strip cast into screed (flush with floor finish)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Dividing strips between differing floor finishes","m",1574,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Standard skimmed metal corner guard, all as per Architectural detail window drawing TYP-042-054 and fixed strictly to manufacturers specification","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Corner guard","m",12054,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TOTAL PLASTERING",null,0,null,{"$f":"SUM(E8165:E8343)","v":{"v":0,"d":"0.00"}}]
[null,null,0,null,{"v":0,"d":"R0.00"}]
["SECTION 2","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NEW HOSPITAL ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D8349*C8349","v":{"v":0,"d":"R0.00"}}]
["BILL NO 13","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TILING","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PREAMBLES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Preambles for Trades as defined in Scope of Work (C3.1 Item 4.1 & Item 4.2)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TRADE NAMES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Any reference to trade names in the Bills of Quantities or  Architect's specification or drawings shall deem to mean \"or similar and approved\"",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["DETAIL DESCRIPTION AND SPECIFICATION","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Note: It is the responsibility of the specialist tiler to study the drawings and design and to allow for\nthe design and execution of special fixing accessories, expansion joints, etc.",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["GENERAL PREAMBLES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Samples - With reference to all items and colour schemes: Samples off all items is to be presented for approval prior to any bulk orders. Please take note that most items will have at least six week delivery period, these approvals will only take place at dates off site meetings, the samples need to be approved well in advance to avoid any delays with lead time on orders. All samples must remain in the sample room for the duration of the contract. Mock up rooms – all wall and floor finishes must be prepared in advance as part of a mock up room/rooms and at least a 100 square meter of vinyl flooring will serve as a sample floor",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 144 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["WALL TILING","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Provide the PC amount of R250/m² supplied and delivered to site for glazed ceramic wall tiles with 2mm joints fixed with approved tile adhesive to plastered walls and waterproof tile grouting to joints (Ref: C2)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On walls","m2",4378,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On partitions","m2",9,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On narrow widths","m2",93,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Provide the PC amount of R250/m² supplied and delivered to site for glazed porcelain wall tiles with 2mm joints fixed with approved tile adhesive to plastered walls and waterproof tile grouting to joints (Ref: C33 & C34)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On walls","m2",2941,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On walls in splash backs","m2",2725,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On narrow widths","m2",92,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["FLOOR TILING","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Provide the PC amount of R400.00/m² supplied and delivered to site for 600 x 600mm Double charged vitrified full body porcelain floor tiles with 2mm wide grouting joints complete with rectangular borders and diagonal infill panels, install with a proprietary tile adhesive as recommended by tile manufacturer on well-prepared screed (elsewhere measured) to suit required level. Finish all joints with a proprietary waterproof grout as recommended by the manufacturer. All strictly to manufacturer’s specifications. Colour and type to Architect’s approval (A3 & A43)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On floors","m2",1736,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On risers 170mm high ","m",2092,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On treads 270mm wide","m",2092,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100mm High cut skirting tile ","m",1751,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100mm High skirting stepped over treads and risers","m",1099,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Provide the PC amount of R450.00/m² supplied and delivered to site for 600 x 600mm Double charged vitrified full body porcelain floor tiles with 2mm wide grouting joints complete with rectangular borders and diagonal infill panels, install with a proprietary tile adhesive as recommended by tile manufacturer on well-prepared screed (elsewhere measured) to suit required level. Finish all joints with a proprietary waterproof grout as recommended by the manufacturer. All strictly to manufacturer’s specifications. Colour and type to Architect’s approval (A49)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On floors","m2",335,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100mm High cut skirting tile ","m",187,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Union Tiles Terra-Stone – Slim Line Terrazzo Rustico cement cement based tiles (Code: 1NUTMEGRSL) or similar approved, size 600 x 600 x 19mm thick  laid externally to 1:50 falls, with 2-5mm joints continuous in both directions grouted with suitable grout (elsewhere specified), excess grout on the surface to be cleaned with water as the work proceeds, bedded in a cement slurry on 25-30mm thick semi-dry mortar screed and tamped using a rubber mallet on a concrete surface bed, conforming to SANS 1200D MJ degree of Accuracy I.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On floors","m2",475,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D8413*C8413","v":{"v":0,"d":"R0.00"}}]
["SUNDRIES","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Aluminium straight edge as by KIRK Marketing (Code: 686) or similar approved","m",6553,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["M-trim aluminium tile stair nosing to suit tile (Code: ATIN100) or similar approved","m",2092,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TOTAL TILING",null,0,null,{"$f":"SUM(E8345:E8419)","v":{"v":0,"d":"0.00"}}]
[null,null,0,null,{"v":0,"d":"R0.00"}]
["SECTION 2","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NEW HOSPITAL ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["BILL NO 14","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["INTERNAL PLUMBING AND DRAINAGE (PROVISIONAL)","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PREAMBLES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Preambles for Trades as defined in Scope of Work (C3.1 Item 4.1 & Item 4.2)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TRADE NAMES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Any reference to trade names in the Bills of Quantities or  Architect's specification or drawings shall deem to mean \"or similar and approved\"",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SUPPLEMENTARY PREAMBLES","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Concrete pipes","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Pipes shall be jointed with interlocking joints",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["UPVC pipes and fittings","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Soil, waste and vent pipes and fittings shall be tempered, chemical resistant pipes with butt welded joints",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["UPVC pressure pipes and fittings","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Pipes for water and fire supply shall be High Impact uPVC of the Class stated",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Pipes shall have cast iron clamped joints. Fittings shall be galvanised mild steel with clamped joints",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Copper pipes","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Pipes shall be hard drawn and half-hard pipes of the class stated. Class 0 (thin walled hard drawn) pipes shall not be bent.  Class 1 (thin walled half-hard), class 2 (half-hard) and Class 3 (heavy walled half-hard) pipes shall only be bent with benders with inner and outer formers, Capillary solder fittings shall comply with ISO 2016. ",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fixing of pipes","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Unless specifically otherwise stated, descriptions of pipes shall be deemed to include fixing to walls etc, casting in, building in or suspending not exceeding 1m below suspension level",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Lead pipes and fittings","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["All soldered joints shall be wiped and brass unions shall be used for jointing lead to steel",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Reducing fittings","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Where fittings have reducing ends or branches they are described as \"reducing\". In the case of pipes with diameters not exceeding 60mm only the largest end or branch size is given. Should the contractor wish to use other fittings and bushes or reducers he may do so on the understanding that no claim in this regard will be entertained. In the case of pipes with diameters exceeding 60mm all sizes are given and no claim for extra bushes, reducers, etc will be entertained",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Wire gratings","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Descriptions of gutter outlets, etc shall be deemed to include wire balloon gratings",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Exposed concrete surfaces","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Exposed surfaces of concrete stormwater channels, cover slabs, inspection eye marker slabs, gulley tops, cleaning eye tops, catchpits, inspection chambers, etc shall be finished smooth with plaster",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D8477*C8477","v":{"v":0,"d":"R0.00"}}]
["Excavations","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["No claim for rock excavation will be entertained unless the contractor has timeously notified the quantity surveyor thereof prior to backfilling",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Soft rock and \"Hard rock\" shall be as defined in \"Earthworks\"",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Laying, backfilling, bedding, etc of pipes","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Pipes shall be laid and bedded and trenches shall be carefully backfilled in accordance with manufacturers' instructions and the Engineer's drawings.",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Where no manufacturers' instructions exist pipes shall be laid in accordance with clauses 5.1 and 5.2 of each of the following:\nSABS 1200 L: Medium-pressure pipelines\nSABS 1200LD: Sewers\nSABS1200LE: Stormwater drainage\nPipe trenches etc shall be backfilled in accordance with clauses 3, 5.5, 5.6, 5.7 and 7 of SABS 1200DB :\nEarthworks (Pipe trenches)\nPipes shall be bedded in accordance with clauses 3.1 to\n3.4.1, 5.1 to 5.3 and 7 of SABS 1200LB : Bedding (Pipes)",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Flush pans","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Flush pans shall have straight or side outlets and \"P\" or \"S\" traps as necessary",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Stainless steel basins, sinks, wash troughs, urinals, etc","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Units shall have standard aprons on all exposed edges and tiling keys against walls where applicable",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Waste unions","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Descriptions of waste unions shall be deemed to include rubber or vulcanite plugs and chains fixed to fittings",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Steel sectional water tanks","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Tanks shall comply with SABS CKS 114",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Petrolatum anti-corrosion tape","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Pipes to be taped shall be coated with the appropriate primer and the tape shall be applied with minimum 15mm lap per spiral unless otherwise described",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Couplings and fittings to pipes shall be taped in strict accordance with the manufacturer's instructions including all mastic, tape, \"Layflat\" sheeting, securing of same, etc",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Prices for wrapping of pipes shall include for all work as described to couplings in the length",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Paper lagging","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Prices for piping must include for all piping not exceeding 30mm to be wrapped with two layers of stout brown paper and tied with wire prior to building in ",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 148 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["RAINWATER DISPOSAL ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["uPVC pipes","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110mm Pipes cast in concrete or built into brickwork","m",208,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110mm Pipes fixed to side of concrete or brickwork","m",3332,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110mm Pipes fixed to underside of concrete ","m",566,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over uPVC pipes for fittings","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110mm Bend","No",1072,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fullbore outlets","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110mm 180 degrees centre bolt concrete roof outlet with dome grating, saint-gabain no 3505 or similar approved","No",278,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["50mm Diameter PVC spout outlet 240mm long cast in concrete beam ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Spout ","No",228,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D8541*C8541","v":{"v":0,"d":"R0.00"}}]
["SANITARY FITTINGS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: All sanitary fittings shall be sealed next to walls, fitting sides and shelves with an approved type non-fungal sustaining white silicon",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["0,9mm Stainless steel type 304 (18/10)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 0,9mm Grade 304 18/10 stainless steel LDL Luxtub (Code: 2560001), size 600 x 500 x 257mm deep with pressed bowl size 525 x 425 x 257mm deep and 40mm waste outlet, Falcon galvanised mild steel bracket with 25mm square mild steel front leg (Code: 2120007) (Code: 2120003) bolted to wall with 6mm anchor bolts or similar approved.","No",11,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["1,2mm Stainless steel type 304 (18/10)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 stainless steel Oval A wash hand basin (Code: 2520029), size 420 x 340 x 185mm deep with a one piece pressed bowl, with two tapholes, 50mm splashback and 100mm radiused apron and 40mm waste outlet, fixed to wall with 4 x 6mm stainless steel anchor bolts or similar approved.","No",170,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 stainless steel PP plaster of paris preparation sink (Code: 2630032), size 1500 x 550 x 1064mm with 525 x 425 x 258mm deep left hand pressed preparation bowl, 150mm high integral splashback, 250 x 535mm deep waste cylinder with stainless steel lid and removable strainer with 40mm waste outlet connected to Cobra chromium plated bottle trap (Code: 345/40), connected to 15mm water supply, fixed to wall and supported on Grade 304 (18/10) stainless steel square gallows brackets with detachable front leg (Code: 2120035), size 40 x 40 x 1,2mm thick, fitted with chrome plated adjustable flanged foot pieces or similar approved.","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 stainless steel P1 pot sinks (Code: 2620481), size 900 x  650 x 1050mm with 760 x 460 x 380mm deep bowl, 150mm high integral splashback to rear, 50 x 10mm turndown and 40mm waste outlet, stainless steel solid undershelf, size 900 x 420mm wide, underside sprayed with vermin proof bitumastic sound deadening, fixed to wall with anchor bolts 900mm from finished floor level and supported on 2No. detachable Grade 304 (18/10) stainless steel round legs (Code: 354700), size 41mm diameter x 1,2mm thick, fitted with chrome plated adjustable flanged foot pieces or similar approved.","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,2mm Grade 304 18/10 stainless steel P2 pot sinks (Code: 2620483), size 2400 x  650 x 1050mm with 2No. 760 x 460 x 380mm deep bowls, 150mm high integral splashback to rear, 50 x 10mm turndown and 40mm waste outlet, stainless steel slatted undershelf (Code: 2620095), size 2400 x 420mm wide, underside sprayed with vermin proof bitumastic sound deadening, fixed to wall with anchor bolts 900mm from finished floor level and supported on Grade 304 (18/10) stainless steel square gallows brackets with detachable front leg (Code: 352654), size 40 x 40 x 1,2mm thick, fitted with chrome plated adjustable flanged foot pieces or similar approved.","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke Grade 304 18/10 stainless steel BR6 bedpan and bottle rack (Code: 2630017) for 6No. pans and 7No. bottles, size 960 x 350 x 500mm with rubber grommets fitted to ends of 8mm diameter bottle rods, removable drip tray with 19mm spigot outlet, fixed to wall with 4No. anchor bolts and flat bar mounting brackets or similar approved.","No",57,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke Trendline Model 1800x535 DCB Grade 304 18/10 polished stainless steel double centre bowl drop on sink (Code: 1030011), overall size 1800 x 535mm with two 343 x 410 x 146mm deep bowls, fitted onto cupboard  (elsewhere specified) or similar approved.","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke Kubus Model KBX 110-20 Austenitic Stainless steel with satin finish single bowl undermount sink (Code: 1220015), overall size 230 x 430mm with one 200 x 400 x 150mm deep bowl, fixed to the underside of  top (elsewhere specified) or similar approved.","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Medhold Medical (011 975 0633) Getinge FD1800 450mm x 580mm x 1320mm Front loaded flusher disinfector used for bedpans and urinals stainless steel chamber internal steam generator rotating and fixed nozzles 3 programs, economy, normal and intensive rinse, wash, disinfect and drying cycles or similar approved.","No",43,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Kwikot Model UTU1000X single end post formed urine test unit size 1000 x 595mm manufactured in 1,2mm grade 304 stainless steel with a 12mm splash back to back, flat top (no fluting) hospital bead only, bowl size 410 x 350 x 150mm deep with a 12mm splashback at rear complete with one PVC combination overflow fitting with anti theft plug or similar approved.","No",12,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Slop Hopper with cowling size 535 x 685 x 510mm high manufactured from 304 (18/10) stainless steel 1.2mm thick with a 100mm high integral splash back to rear and both sides. The cone has integral flushing rim and 100mm Diameter stainless steel S or P trap. Unit fitted with a back entry flush pipe for a standard flush valve. Unit fitted with a hinged bucket grid manufactured from 10mm diameter 304 (18/10) complete with two 40 x 40mm square stainless steel wall mounting gallows brackets fixed with 4 of anchor bolts. Slop hopper supplied complete with floor mounting bracket as per manufacturers specification","No",37,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Single centre bowl special post formed sink size 900 x 595mm manufactured in 1.2mm grade 304 stainless steel bowl size 410 x 350 x 150mm deep with a 12mm splashback at rear complete with PVC combination overflow fitting with anti theft plug and back entry spreader fitted to bowl on right hand side.","No",129,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Double end special post formed sink size 1200 x 595 manufactured in 1.2mm grade 304 stainless steel bowl size 410 x 350 x 150mm deep single left hand bowl sink with a 12mm splashback at rear complete with PVC combination overflow fitting with anti theft plug and back entry spreader fitted to bowl on right hand side.","No",92,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Double centre bowl special post formed sink size 1600 x 595 manufactured in 1.2mm grade 304 stainless steel bowl size 410 x 350 x 150mm deep single left hand bowl sink with a 12mm splashback at rear complete with PVC combination overflow fitting with anti theft plug and back entry spreader fitted to bowl on right hand side.","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["1,6mm Stainless steel type 304 (18/10)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,6mm Grade 304 18/10 stainless steel SMS surgeon mini scub-up unit (Code: 2630049), size 665 x 554 x 561mm with 525 x 425 x 258mm deep pressed bowl, 300mm high integral splashback, 2No. 22mm tap holes, 90mm waste outlet, basket strainer fitting, connected to 15mm water supply, fixed to removable 1,6mm thick galvanised mild steel fixing plate and bolted to wall with anchor bolts 900mm from finished floor level or similar approved.","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,6mm Grade 304 18/10 stainless steel SSW12 hospital surgeon scrub-up unit (Code: 2630044), size 1200 x 460 x 555mm with radiused internal corners, front and side of unit to be of double walled construction with inner wall sprayed with vermin proof bitumastic sound deadening approximately 2mm thick, 150mm high integral splashback, 40mm waste outlet connected to Cobra chromium plated bottle trap (Code: 345/40), connected to 15mm water supply, fixed tor emovable 2mm thick galvanised mild steel fixing plate and bolted to wall with anchor bolts 900mm from finished floor level or similar approved.","No",20,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,6mm Grade 304 18/10 stainless steel SSW15 hospital surgeon scrub-up unit (Code: 2630045), size 1500 x 460 x 555mm with radiused internal corners, front and side of unit to be of double walled construction with inner wall sprayed with vermin proof bitumastic sound deadening approximately 2mm thick, 150mm high integral splashback, 40mm waste outlet connected to Cobra chromium plated bottle trap (Code: 345/40), connected to 15mm water supply, fixed tor emovable 2mm thick galvanised mild steel fixing plate and bolted to wall with anchor bolts 900mm from finished floor level or similar approved.","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,6mm Grade 304 18/10 stainless steel SSW18 hospital surgeon scrub-up unit (Code: 2630046), size 1800 x 460 x 555mm with radiused internal corners, front and side of unit to be of double walled construction with inner wall sprayed with vermin proof bitumastic sound deadening approximately 2mm thick, 150mm high integral splashback, 2No. 40mm waste outlets connected to Cobra chromium plated bottle trap (Code: 345/40), connected to 15mm water supply, fixed tor emovable 2mm thick galvanised mild steel fixing plate and bolted to wall with anchor bolts 900mm from finished floor level or similar approved.","No",17,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,6mm Grade 304 18/10 stainless steel EL bedpan sluice sink (Code: 2630012), size 1130 x 685 x 1050mm with right hand pressed seamless sluice bowl with integral flushing rim, 150mm high integral splashback, 15mm deep hospital bead, 100mm apron, 110mm waste outlet connected to S or P trap (elsewhere specified), unit supplied complete with factory fitted Cobra FM 1,00 flush valve connected to 35mm water supply, 15mm bedpan and bottle spray nozzle activated by 2No 15mm quarter turn elbow action valves, fixed to wall and supported on Grade 304 (18/10) stainless steel square gallows brackets with detachable front leg (Code: 2120035), size 40 x 40 x 1,2mm thick, fitted with chrome plated adjustable flanged foot pieces or similar approved.","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 1,6mm Grade 304 18/10 stainless steel EC6 combination bedpan and wash-up sink (Code: 2630002), size 1830 x 685mm with one pressed seamless sluice bowl with integral flushing rim and one 610 x 460 x 230mm deep left hand pressed seamless rinse bowl, 150mm high integral splashback, 15mm deep hospital bead, 100mm apron, 110mm waste outlet connected to S or P trap (elsewhere specified) on sluice bowl and 40mm waste outlet connected to Cobra chromium plated bottle trap (Code: 345/40) on rinse bowl, unit supplied complete with factory fitted Cobra FM 1,00 flush valve connected to 35mm water supply, CP171/041 pillar mixer with over-arm swivel spout, CP297 pillar mixer with retractable hand spray, 15mm bedpan and bottle spray nozzle activated by 2No 15mm quarter turn elbow action valves, fixed to wall and supported on Grade 304 (18/10) stainless steel square gallows brackets with detachable front leg (Code: 2120035), size 40 x 40 x 1,2mm thick, fitted with chrome plated adjustable flanged foot pieces or similar approved.","No",56,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["White glazed vitreous china","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Vaal Sanitaryware Sola 630 fine fireclay wall hung basin colour White (Code: 702800WH), overall size 630 x 500 x 200mm without tapholes, bolted to wall with concealed wall bracket (Code: 8131Z300) and 4No.10mm bolts (Code: 8448Z000) and sealed with silicone sealant where basin meets wall or similar approved.","No",647,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Vaal Sanitaryware Lab Sink ceramic fireclay laboratory sink colour White (code: 234500), size 435 x 335mm with waste outlet including acid resistant waste fitting (code: 8790Z000) fitted underneath opening in worktop surface (by others) on and including two adjustable under slung brackets (code: 8109Z000) or similar approved.","No",16,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Vaal Sanitaryware Hibiscus vitreous china wall hung basin colour White (Code: 702303WH), overall size 510 x 405mm with two tapholes including integrated overflow and chainstay hole, bolted to wall with 2No.10mm bolts (Code: 8448Z000) and sealed with silicone sealant where basin meets wall or similar approved.","No",351,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Vaal Sanitaryware Concorde Slimline vitreous china self-rimming drop-in basin colour White (Code: 704700WH), overall size 590 x 390 x 180mm, sealed with silicone sealant, all in accordance with the manufacturer's specifications or similar approved.","No",63,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Vaal Sanitaryware Bantam vitreous china cloakroom basin colour White (Code: 703003WH), overall size 455 x 290 x 210mm with two tapholes including integrated overflow and chainstay hole, bolted to wall with 2No.10mm bolts (Code: 8448Z000) and sealed with silicone sealant where basin meets wall or similar approved.","No",97,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Vaal Sanitaryware Entice vitreous china 90° outlet back inlet rimless back to wall toilet colour White (Code: 431300WH), overall size 350 x 400 x 570mm high with quality thermoset soft close seat and floor brackets with concealed back inlet flushvalve (elsewhere specified) or similar approved.","No",237,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D8605*C8605","v":{"v":0,"d":"R0.00"}}]
["Vaal Sanitaryware Protea Paraplegic washdown suite comprising 90° outlet open rim pan (code: 750246WH) including lid and fitments with heavy duty seat or similar approved.","No",254,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Vaal Sanitaryware 600 x 385 x 380mm Lavatera white vitreous china wall mounted urinal (Code: 705427WH) including 38mm chromium plated domical grating (Code: 8787Z0) and chromium plated back inlet spreader (Code: 7054Z2), fixed on and including two hanger brackets (Code: 8127Z0) or similar approved.","No",17,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cobra salon basin semi recessed 470mm x 500mm (Code: COB-VSI-SAL-050-NA-L-WHI) or similar approved.","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Purpose made washbowl size525 x 370 x 115mm deep complete with under mounted hand washbowl (bowl product code WAVONITELOVALBWL), all in accordance with the manufacturer's specifications. (Max on Top 082 789 3580) or similar approved.","No",15,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Vandal Resistant Sanitaryware Whyte house security pan WHPP-3 (1705) bolted and epoxy grout to wall, all in accordance with the manufacturer's specifications or similar approved. ","No",29,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Vandal Resistant Sanitaryware Whyte house basin WHBMK11-6 (1705) with two tap holes, complete with Wirquin trap as recommended by manufacturers, bolted and epoxy grout to wall, all in accordance with the manufacturer's specifications or similar approved.","No",32,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Vandal Resistant Sanitaryware Whyte house urinal WHU-9 (1711)  with flushing valve (elsewhere), complete with Wirquin trap as recommended by manufacturers, bolted and epoxy grout to wall, all in accordance with the manufacturer's specifications or similar approved.","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Baths","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Plexicor Carmen 1200 rectangular bath BRC-CAR-120-NH-L-WHI, with seat, overall size 1200 x 700 x 390mm high supported on 38 x 38mm timber battens fixed to adjacent walls and bed in 1:5 cement mortar on a brick bed, three bricks wide for full length of bath with the void between the bath and enclosing wall filled with 1:10 uncompacted cement mix and point all round with mildew resistant silicone between bath and tiles, all in accordance with the manufacturer's specifications or similar approved.","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Plexicor Alexa 1800 acrylic bath with integrated arm rests in colour White, overall size 1800 x 900 x 460mm high supported on 38 x 38mm timber battens fixed to adjacent walls and bed in 1:5 cement mortar on a brick bed, three bricks wide for full length of bath with the void between the bath and enclosing wall filled with 1:10 uncompacted cement mix and point all round with mildew resistant silicone between bath and tiles, all in accordance with the manufacturer's specifications or similar approved.","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Purpose made baby bath size 680 x 430 x 175mm overall high from Avonite Solid Surfacing integrated into solid surface top complete with under mounted bath (bath product code WAVONITEBABYBATH ), all in accordance with the manufacturer's specifications. (Max on Top 082 789 3580) or similar approved.","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Shower Trolley (Code: BAB5000-01) complete with thermostatic mixer for shower and disinfection with flush valve (Code: BCA1221-04) and flush sink of stainless steel S-trap (Code: 080015-54) (Arjo Huntleigh 012-527 2000) or similar approved.","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["WASTE UNIONS, ETC","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Chromium plated","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
[" 32mm Unslotted waste (Code: 308) with 62mm diameter flange, 80mm long shank and plug.","No",47,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
[" 32mm Unslotted waste (Code: 308) with 62mm diameter flange, 80mm long shank with backnut, anti-theft plug (code: 309-32)","No",713,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["32mm Slotted waste (Code: 303) with 62mm diameter flange, 80mm long shank with backnut, anti-theft plug (code: 309-32)","No",448,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["40mm Chrome plated slotted waste (Code: 316) with 70mm diameter flange, 45mm long shank, plug, chain and stay.","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["40mm Chrome plated unslotted waste (Code: 317-40) with 70mm diameter flange, 45mm long shank, plug, chain and stay.","No",251,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["40mm Chrome plated unslotted waste (Code: 317-40) with 70mm diameter flange, 45mm long shank with backnut, anti-theft plug (code: 309-32)","No",351,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["40mm Chrome plated anti-theft plug (code: 309-40)","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Stainless Steel","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Polydrain ACO shower drain with 50mm side outlet stainless steel drain body with removable foul air trap and nylon vinyl clamps (Code: 405819) including grade 304 stainless steel perforated grating (Code: 403234), connected to 50mm waste pipe, installed with the manufacturer`s recommendations or similar approved.","No",207,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Polydrain ACO shower drain with 50mm side outlet stainless steel drain body with removable foul air trap and nylon vinyl clamps (Code: 405821) including grade 304 stainless steel perforated grating (Code: 405156), connected to 50mm waste pipe, installed with the manufacturer`s recommendations or similar approved.","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Rofo Engineering grade AISI 304 stainless steel RO 200 NW 100 floor drain with square top flange and square cover plate with circular aperture (Code: RO200VNW100SQ - circular) cast into floor slab to be flush with the floor finish (floor finish to be sloped towards floor drains), overall size 240mm x 220mm deep, with 110mm diameter vertical waste outlet connected to waste pipe. All installed strictly to manufacturers specifications (FD001) or similar approved.","No",7,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Rofo Engineering grade AISI 304 stainless steel RO 280 NW 100 floor drain with square top flange and square cover plate with circular aperture (Code: RO200VNW100SQ - circular) cast into floor slab to be flush with the floor finish (floor finish to be sloped towards floor drains), overall size 310mm x 230mm deep, with 110mm diameter vertical waste outlet connected to waste pipe. All installed strictly to manufacturers specifications (FD002) or similar approved.","No",8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Rofo Engineering grade AISI 304 stainless steel ROC 250 straight floor channel with stainless steel grating cast into floor slab to be flush with the floor finish (floor finish to be sloped towards floor drains), overall size 1000mm long x 350mm wide x 200mm deep including RO 200V NW 100 floor drain positioned in the side of channel with 100mm waste outlet connected to waste pipe. All installed strictly to manufacturers specifications (FD003) or similar approved.","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TRAPS, ETC","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Rubber","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["40mm Combination overflow and waste ","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Brass","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["40mm Shallow seal bath P trap with FI outlet and two cleaning eyes","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D8669*C8669","v":{"v":0,"d":"R0.00"}}]
["Chromium plated","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["40mm Deep seal bottle trap with outlet for 50mm PVC (code: 345/50)","No",1176,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["40mm Deep seal bottle trap with outlet for 50mm PVC (code: 365/50)","No",622,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TAPS, VALVES, ETC","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sundries","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cobra Watertech Carina Chrome pillar tap (Code: 114CA-15), manufactured in accordance with SANS 226 Type 2, installed in accordance with the manufacturers recommendations or similar approved.","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cobra Watertech Carina Chrome sink mixer, with retractable hand spray (Code: 297CA), installed in accordance with the manufacturers recommendations or similar approved.","No",55,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cobra Watertech Carina Chrome pillar type sink mixer, (Code: 171/041CA), installed in accordance with the manufacturers recommendations or similar approved.","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cobra Watertech Cobratron Chrome electronic mixer (Code: EL-508UNDER), installed in accordance with the manufacturers recommendations or similar approved.","No",43,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cobra Watertech Stella Chrome pillar tap (Code: 3314ST-15), manufactured in accordance with SANS 226 Type 2, installed in accordance with the manufacturers recommendations or similar approved.","No",328,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cobra Watertech Stella Chrome pillar tap (Code: 3294ST-15), manufactured in accordance with SANS 226 Type 2, installed in accordance with the manufacturers recommendations or similar approved.","No",65,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cobra Watertech Stella Chrome one hole sink mixer (Code: 3396ST), manufactured in accordance with SANS 226 Type 2, installed in accordance with the manufacturers recommendations or similar approved.","No",240,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cobra Watertech Stella Chrome shower under wall stop tap (Code: 3338ST-15), manufactured in accordance with SANS 226 Type 2, installed in accordance with the manufacturers recommendations or similar approved.","No",80,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cobra Watertech Stella Chrome extended bibtap (Code: 3306ST/EXT-15), manufactured in accordance with SANS 226 Type 2, installed in accordance with the manufacturers recommendations or similar approved.","No",74,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cobra Watertech Stella Chrome bibtap (Code: 3306ST-15), manufactured in accordance with SANS 226 Type 2, installed in accordance with the manufacturers recommendations or similar approved.","No",22,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cobra Watertech Stella Chrome bibtap (Code: 3309ST), manufactured in accordance with SANS 226 Type 2, installed in accordance with the manufacturers recommendations or similar approved.","No",86,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cobra Watertech Star 15mm Chrome plated bibtap (code: 107EC-15), installed in accordance with the manufacturers recommendations or similar approved.","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cobra Watertech Chrome shower arm (Code:026), size 68mm long or similar approved.","No",22,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cobra Watertech Chrome shower rose (Code:KP2.51) or similar approved.","No",22,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cobra Watertech Medical Elbow Action Chrome medical mixer (Code: 510-21), manufactured in accordance with SANS 226 Type 2, installed in accordance with the manufacturers recommendations or similar approved.","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cobra Watertech Medical Elbow Action pillar-type mixer with swan-neck swivel outlet (Code: 515-21), manufactured in accordance with SANS 226 Type 2, installed in accordance with the manufacturers recommendations or similar approved.","No",13,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cobra Watertech Medical Elbow Action wall-type mixer with aerated swan-neck swivel outlet (Code: 515/055-21), manufactured in accordance with SANS 226 Type 2, installed in accordance with the manufacturers recommendations or similar approved.","No",647,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Walker Croswellar, Rada 320 OEM thermostatic mixing valve complete hose station with Rada 320 OEM thermostatic mixing valve, 15meters 20mm hose, hose rack and hose trigger gun as by Walker Crosweller. Installed strictly to manufacturers specifications or similar approved.","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Walker Croswellar, Walcro CIRS-V3-6 vandal resistant shower rose, chrome finish. Installed strictly to manufacturers specifications or similar approved.","No",18,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["20mm Chromium plated Strata built-in thermostatic shower mixer with cover plate (Code: SA-862MEDI) or similar approved.","No",190,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cobra Watertech Chrome Standard Flushmaster exposed toilet flush valve (Code: FJ2-210), installed in accordance with the manufacturer`s recommendations or similar approved.","No",37,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cobra Watertech exposed urinal chrome plated Junior Econo Flushmaster flushvalve (code: KF8.112) with non-hold open feature, galvanised steel undertile box with stainless steel faceplate and chasis, palm press button, 22mm diameter copper urinal tailpipe and 20mm \"Ball-o-stop\" control inlet, installed in accordance with the manufacturer`s recommendations or similar approved.","No",21,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cobra Watertech exposed WC chrome plated Junior Flushmaster flushvalve (code: KF4.213) with non-hold open feature, vacuum breaker, back entry flushpipe, galvanised steel undertile box with stainless steel faceplate and chasis, palm press button, rubber pan connector and 32mm \"Ball-o-stop\" control inlet, installed in accordance with the manufacturer`s recommendations or similar approved.","No",517,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cobra Watertech Chrome hand shower (Code:07V/CP) with two spray functions (classic jet and champagne spray) and removable water-saving insert or similar approved.","No",187,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cobra Watertech Chrome hand shower (Code:07MJ/CP) with four spray functions (classic jet, tropical mist, classic jet and tropical mist combined, and pause) and anti-lime nipples or similar approved.","No",187,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cobra Watertech Chrome hand shower hose (Code:008/7), size 1250mm long or similar approved.","No",187,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cobra Watertech Chrome shower rail set (Code:002/1), size 550mm long with sliding hand shower holder or similar approved.","No",187,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D8733*C8733","v":{"v":0,"d":"R0.00"}}]
["Cobra Watertech Chrome wall outlet (Code:AP8-311) with wall outlet elbow or similar approved.","No",181,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cobra Watertech Chrome hand spray (Code:C-017) with single function classic jet spray and aerated flow or similar approved.","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cobra Watertech Chrome hand shower hose (Code:008CO), size 950mm long or similar approved.","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["15mm Chrome ball type angle valve (Code: 832/350F). Including 350mm braided flexi hose or similar approved.","No",1550,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["15mm Chrome ball type angle valve (Code: 232/350). Including 350mm pipe or similar approved. ","No",338,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cobra Watertech Medical Elbow Action Chrome pillar tap (Code: 505-21B), manufactured in accordance with SANS 226 Type 2, installed in accordance with the manufacturers recommendations or similar approved.","No",458,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cobra Watertech Medical Elbow Action Chrome pillar tap (Code: 505-21R), manufactured in accordance with SANS 226 Type 2, installed in accordance with the manufacturers recommendations or similar approved.","No",458,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cobra Watertech Medical Elbow Action Chrome side valve (Code: 514-21B), manufactured in accordance with SANS 226 Type 2, installed in accordance with the manufacturers recommendations or similar approved.","No",116,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cobra Watertech 19 x 160mm Chrome plated diverter bath spout with round wall flange (067S). Including female inlet with 160mm throw, sliding wall flange, diversion mechanism for diversion to hand shower attachment, and hand shower, installed in accordance with the manufacturers recommendations or similar approved.","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cobra Watertech 15mm chrome plated concealed WAVE SWITCH sensor (Code: EL-3012-Wcp) with \"4\"x4\" Galvanise Box, Adjustable Galvanise Yolk and Stainless Steel Cover Plate. Complete with Sensor, Solenoid and 240V to 9V Transformer, installed in accordance with the manufacturers recommendations or similar approved.","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Broen Bench Mounted one hole mixer with swivel spout and detachable nozzle (Code: 2536 039 1039-52E), installed in accordance with the manufacturers recommendations or similar approved.","No",16,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Broen wall mounted eye shower with two 45 degree angled heads, including 1500mm inlet hose. Trigger operated including check valve and flowfix for regulation of water flow (Code: 27 1000.9100.3011), installed in accordance with the manufacturers recommendations or similar approved.","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Broen body shower, ceiling mounted with self-draining head. In brass with chemical resistant Broen-lab polycoat. Minimum 1 bar working pressure. (Code: 17 580.709), installed in accordance with the manufacturers recommendations or similar approved.","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Body shower with eye/face shower and bowl, modular. In brass and SS with chemical resistant red BROEN-LAB Polycoat with self-draining shower head. Eye wash with built-in FLOWFIX for regulation of water flow (16 l/min). Bowl in Stainless Steel with integrated outlet, installed in accordance with the manufacturers recommendations or similar approved.","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["20mm Hose bibtap brass (code: 309-20) or similar approved.","No",118,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Libra Premier Combo factory installed spa conversion consisting of air channel, 10 x aeration floor jets, 6 x hydro jets, remote pop-up waste with built in filler spout and supply and site installation of aeration blower, 1,0hp jet pump and pneumatic on/off control switch, 2 x control electronic switch, run dry protection, in-line heater, 1 x chrome hydro jet. Spa to be connected to 50mm waste outlet and wastepipe, 15mm cold water supply (by others) and single phase electrical power supply (by others) or similar approved.","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SANITARY PIPEWORK","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["HDPE PN 4  soil and waste pipes in trenches for use above ground in accordance with SABS 791 ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["56mm Pipes ","m",12,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110mm Pipes ","m",68,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra on HDPE pipes for:","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["56mm Bend","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["56mm Junction ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110mm Bend ","No",15,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110mm Junction ","No",11,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110mm Rodding eye ","No",8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110 x 50mm Reducer","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110 x 50mm Reducing junction","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Inherent Co-Polymer Polyproylene soil and waste pipes Heavy duty Class 51 for use above ground in accordance with SABS 791 ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["50mm Pipes fixed to concrete soffits  ","m",49,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110mm Pipes fixed to concrete soffits  ","m",36,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over Inherent Co-Polymer Polyproylene pipes for fittings","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D8797*C8797","v":{"v":0,"d":"R0.00"}}]
["50mm Bend ","No",19,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["50mm Tee","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110mm Bend ","No",29,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110mm Junction ","No",36,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110mm Rodding eye ","No",10,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110 x 50mm Reducer","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110 x 50mm Reducing junction","No",9,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["160mm Junction ","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["160 x 110mm Reducer","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Inherent Co-Polymer Polyproylene soil and waste pipes Heavy duty Class 34 for use under ground in accordance with SABS 791 with uPVC couplings with and including excavation, bedding material, back filling, compaction, etc.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110mm Pipes laid in and including trenches not exceeding 1m deep under surface beds ","m",216,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["160mm Pipes laid in and including trenches not exceeding 1m deep under surface beds ","m",12,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["uPVC PN 1 soil and waste pipes Heavy duty Class 51 for use above ground in accordance with SABS 791 ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["25mm Pipes fixed to concrete soffits  ","m",108,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["50mm Pipes","m",8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["50mm Pipes in walls ","m",1043,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["50mm Pipes fixed to concrete soffits  ","m",7439,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["75mm Pipes","m",33,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["75mm Pipes fixed to concrete soffits  ","m",482,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110mm Pipes","m",1315,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110mm Pipes fixed to concrete soffits  ","m",7851,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["160mm Pipes ","m",331,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["160mm Pipes fixed to concrete soffits  ","m",560,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["uPVC PN 3 soil and waste pipes Heavy duty Class 34 for use under ground in accordance with SABS 791 with uPVC couplings with and including excavation, bedding material, back filling, compaction, etc.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["50mm Pipes laid in and including trenches not exceeding 1m deep under surface beds ","m",22,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110mm Pipes laid in and including trenches not exceeding 1m deep under surface beds ","m",3281,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over uPVC pipes for fittings","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["25mm Bend ","No",18,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["50mm Bend ","No",3343,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["50mm Access bend ","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["50 x 25mm Reducer ","No",9,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["50mm Rodding eye","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D8861*C8861","v":{"v":0,"d":"R0.00"}}]
["50mm Tee","No",390,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["50mm Junction","No",90,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["75mm Bend","No",77,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["75mm Tee","No",16,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["75mm Y junction","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["75 x 50mm Reducer ","No",13,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["75 x 75 x 50mm Reducing junction ","No",12,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110mm Bend ","No",2092,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110mm Access bend ","No",202,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110mm Junction ","No",1520,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110mm Y Junction ","No",28,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110mm Access junction ","No",164,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110mm Straight pan connector ","No",491,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110mm Rodding eye ","No",1027,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110mm Vent valve ","No",100,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110 x 50mm Reducer","No",174,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110 x 75mm Reducer","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110 x 50mm Reducing junction","No",1033,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110 x 50mm Access reducing junction","No",23,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110mm End cap","No",8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["160mm Bend ","No",256,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["160mm Junction ","No",164,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["160 x 110mm Reducer","No",82,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["160 x 110mm Reducing junction ","No",400,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["160mm Rodding eye","No",46,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Gulleys","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Gulley not exceeding 1m deep to invert comprising 110mm diameter uPVC gulley trap and head, fitted with 190mm diameter cast iron grating, including excavating for, bedding on and encasing in 15MPa/19mm mass concrete and fitted with and including precast gulley top bedded in cement mortar, including 100mm gulley head","No",22,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TESTING","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Testing sewer system","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["WATER SUPPLY","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Galvanised steel pipes","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["80mm Pipes","m",9,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D8925*C8925","v":{"v":0,"d":"R0.00"}}]
["100mm Pipes","m",234,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["125mm Pipes","m",73,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150mm Pipes","m",67,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["250mm Pipes","m",29,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over galvanised steel pipes for flanged steel fittings","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["80mm Bend","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100mm Bend ","No",88,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["125mm Bend  ","No",10,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["125 x 80 x 80mm Reducing tee ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["125 x 125 x 80mm Reducing tee ","No",9,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150mm Bend","No",15,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150mm Tee","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["250mm Bend","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Taps, Valves, etc.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100mm Brass Shut -off  valve jointed to galvanised pipe including adaptors","No",25,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["125mm Brass Shut -off  valve jointed to galvanised pipe including adaptors","No",8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["200mm Brass Shut -off  valve jointed to galvanised pipe including adaptors","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["250mm Brass Shut -off  valve jointed to galvanised pipe including adaptors","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100mm Brass adjustable PRV with pressure gauge to galvanised pipe including adaptors","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["125mm Brass adjustable PRV with pressure gauge to galvanised pipe including adaptors","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["125mm Brass spring loaded non- return valve to galvanised pipe including adaptors","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["125mm Scour valve to galvanised pipe including adaptors","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["HDPE PN 12.5 pipes in trenches for use under ground in accordance with SABS 791 with compression fittings with and including excavation, bedding material, back filling, compaction, etc.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["15mm Diameter pipe not exceeding 1m deep","m",11,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["20mm Diameter pipe not exceeding 1m deep","m",13,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["32mm Diameter pipe not exceeding 1m deep","m",266,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["HDPE PN 16 pipes in trenches for use under ground in accordance with SABS 791 with compression fittings with and including excavation, bedding material, back filling, compaction, etc.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["63mm Diameter pipe not exceeding 1m deep","m",83,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["HDPE PN 16 pipes in accordance with SABS 791 with compression fittings, etc.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["32mm Diameter pipe","m",186,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["75mm Diameter pipe","m",2531,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110mm Diameter pipe","m",388,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D8989*C8989","v":{"v":0,"d":"R0.00"}}]
["Extra on HDPE pipes for:","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["32mm HDPE bend","No",261,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["32mm HDPE tee","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["75mm HDPE bend","No",346,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["75mm HDPE tee","No",45,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["75 x 32mm HDPE reducer","No",44,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["75 x 75 x 32mm HDPE reducing tee","No",68,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110mm HDPE bend","No",13,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110 x 110 x 32mm HDPE reducing tee","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110 x 110 x 75mm HDPE reducing tee","No",11,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Taps, Valves, etc.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["80mm Brass Shut -off  valve jointed to HDPE pipe including adaptors","No",23,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100mm Butterfly valve jointed to HDPE pipe including adaptors","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Class 1 copper pipes for capillary fittings in accordance with SABS 460 ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["15mm Pipes ","m",10032,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["15mm Pipes chased into brickwork including wrapping ","m",10020,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["22mm Pipes ","m",695,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["22mm Pipes  chased into brickwork including wrapping ","m",310,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["28mm Pipes ","m",1490,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["28mm Pipes chased into brickwork including wrapping ","m",80,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["35mm Pipes ","m",2908,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["35mm Pipes chased into brickwork including wrapping ","m",1470,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["42mm Pipes ","m",7482,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["54mm Pipes ","m",6842,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["67mm Pipes ","m",4425,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["76mm Pipes ","m",9135,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["108mm Pipes ","m",2803,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over for fittings","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over Class 1 copper pipes for brass capillary soldered fittings ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["15mm Fittings","No",19408,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["22mm Fittings","No",1149,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["28mm Fittings","No",523,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D9053*C9053","v":{"v":0,"d":"R0.00"}}]
["35mm Bend","No",2378,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["35mm Tee ","No",597,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["35 x 15mm Reducer ","No",766,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["35 x 22mm Reducer ","No",17,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["35 x 28mm Reducer ","No",10,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["35 x 35 x 15mm Reducing tee ","No",290,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["35 x 35 x 22mm Reducing tee ","No",18,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["35 x 35 x 28mm Reducing tee ","No",11,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["42mm Bend","No",1043,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["42mm Tee","No",50,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["42mm Cross","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["42 x 15mm Reducer ","No",16,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["42 x 22mm Reducer ","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["42 x 28mm Reducer ","No",34,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["42 x 35mm Reducer ","No",29,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["42 x 42 x 15mm Reducing tee ","No",712,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["42 x 42 x 22mm Reducing tee ","No",56,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["42 x 42 x 28mm Reducing tee ","No",10,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["42 x 42 x 35mm Reducing tee ","No",29,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["54mm Bend","No",941,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["54mm Tee ","No",593,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["54 x 54 x 22mm Reducing tee ","No",37,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["54 x 54 x 28mm Reducing tee ","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["54 x 54 x 35mm Reducing tee ","No",13,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["54 x 54 x 42mm Reducing tee ","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["54 x 15mm Reducer ","No",558,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["54 x 28mm Reducer ","No",20,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["54 x 35mm Reducer ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["54 x 42mm Reducer ","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["67mm Bend","No",584,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["67mm Tee ","No",378,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["67 x 67 x 28mm Reducing tee ","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D9117*C9117","v":{"v":0,"d":"R0.00"}}]
["67 x 67 x 35mm Reducing tee ","No",130,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["67 x 67 x 42mm Reducing tee ","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["67 x 67 x 54mm Reducing tee ","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["67 x 15mm Reducer","No",322,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["67 x 22mm Reducer","No",10,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["67 x 28mm Reducer","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["67 x 35mm Reducer","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["76mm Bend","No",1325,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["76mm Tee ","No",762,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["76 x 76 x 28mm Reducing tee ","No",9,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["76 x 76 x 35mm Reducing tee ","No",308,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["76 x 76 x 42mm Reducing tee ","No",9,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["76 x 76 x 54mm Reducing tee ","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["76 x 76 x 67mm Reducing tee ","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["76 x 15mm Reducer","No",673,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["76 x 22mm Reducer","No",44,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["76 x 42mm Reducer","No",13,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["76 x 67mm Reducer","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["108mm Bend","No",46,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["108 x 108 x 54mm Reducing tee","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Taps, Valves, etc.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["15mm Brass Shut -off valve jointed to copper pipe including adaptors","No",3078,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["20mm Brass Shut- off  valve jointed to copper pipe including adaptors","No",144,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["25mm Brass Shut- off  valve jointed to copper pipe including adaptors","No",510,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["32mm Brass Shut -off  valve jointed to copper pipe including adaptors","No",529,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["35mm Brass Shut -off  valve jointed to copper pipe including adaptors","No",41,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["40mm Brass Shut -off  valve jointed to copper pipe including adaptors","No",168,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["40mm Lockable Brass Shut -off  valve jointed to copper pipe including adaptors","No",433,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["42mm Brass Shut -off  valve jointed to copper pipe including adaptors","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["50mm Brass Shut -off  valve jointed to copper pipe including adaptors","No",86,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["50mm Lockable Brass Shut -off  valve jointed to copper pipe including adaptors","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["65mm Brass Shut -off  valve jointed to copper pipe including adaptors","No",324,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D9181*C9181","v":{"v":0,"d":"R0.00"}}]
["76mm Brass Shut -off  valve jointed to copper pipe including adaptors","No",225,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["20mm Brass adjustable PRV with pressure gauge to copper pipe including adaptors","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["25mm Brass adjustable PRV with pressure gauge to copper pipe including adaptors","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["32mm Brass adjustable PRV with pressure gauge to copper pipe including adaptors","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["40mm Brass adjustable PRV with pressure gauge to copper pipe including adaptors","No",83,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["50mm Brass adjustable PRV with pressure gauge to copper pipe including adaptors","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["65mm Brass adjustable PRV with pressure gauge to copper pipe including adaptors","No",48,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["80mm Brass adjustable PRV with pressure gauge to copper pipe including adaptors","No",32,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["15mm Brass spring loaded non- return valve to copper pipe including adaptors","No",454,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["20mm Brass spring loaded non- return valve to copper pipe including adaptors","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["25mm Brass spring loaded non- return valve to copper pipe including adaptors","No",83,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["32mm Brass spring loaded non- return valve to copper pipe including adaptors","No",8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["40mm Brass spring loaded non- return valve to copper pipe including adaptors","No",163,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["50mm Brass spring loaded non- return valve to copper pipe including adaptors","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["65mm Brass spring loaded non- return valve to copper pipe including adaptors","No",96,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["80mm Brass spring loaded non- return valve to copper pipe including adaptors","No",64,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["20mm Scour Valve to copper pipe including adaptors","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["25mm Scour Valve to copper pipe including adaptors","No",83,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["32mm Scour Valve to copper pipe including adaptors","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["40mm Scour Valve to copper pipe including adaptors","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["50mm Scour Valve to copper pipe including adaptors","No",84,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["65mm Scour Valve to copper pipe including adaptors","No",80,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["15mm Brass thermostatic mixing valve to copper pipe including adaptors","No",227,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["25mm Air release Valve to copper pipe including adaptors","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["32mm Vacuum breaker valve to copper pipe including adaptors","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["50mm Water flow meter to copper pipe including adaptors","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["80mm Flow balancing valve to copper pipe including adaptors","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["LAGGING","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Polyethylene closed cell elastomeric insulation such as k-flex to an R1 rating per SANS 10252-1 or equal and approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Insulation to 15mm pipe and couplings","m",5017,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Insulation to 22mm pipe and couplings","m",429,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Insulation to 28mm pipe and couplings","m",1318,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D9245*C9245","v":{"v":0,"d":"R0.00"}}]
["Insulation to 35mm pipe and couplings","m",664,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Insulation to 42mm pipe and couplings","m",6702,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Insulation to 54mm pipe and couplings","m",5889,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Insulation to 67mm pipe and couplings","m",238,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Insulation to 108mm pipe and couplings","m",1318,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Preformed mineral glass wool insulation with aluminium foil wrap to an R1 rating per SANS 10252-1 or equal and approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["65mm Insulation to 54mm pipe and couplings","m",239,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["65mm Insulation to 67mm pipe and couplings","m",20,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["65mm Insulation to 76mm pipe and couplings","m",73,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["65mm Insulation to 80mm pipe and couplings","m",9,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["65mm Insulation to 108mm pipe and couplings","m",88,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["65mm Insulation to 125mm pipe and couplings","m",57,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TESTING","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Pressure testing water pipe system","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["ELECTRIC WATER HEATERS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Hydroboil or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Zip stainless steel 7,5 litre Hydroboil (Code: 2610291), size 318 x 198 x 578mm high with instant boiling water, two way tap control, connected to 15mm cold water supply with service valve, waste for safety valve connected to waste water system and 220 volt 15 amp electrical power supply, plugged and screwed to wall and fitted under 1 year guarantee.","No",109,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["DOMESTIC HOT WATER SYSTEM  ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Hot Tanks","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Heat accumulator c/w tank float valve, filling station, 3 sensor pockets, insulation and cladding and 36 kW electrical resistance elements. Refer to Part C3.3 Hot water storage tanks","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Heat accumulator, 11m³, T-03, low pressure thermal hot water tank, incorporating a high pressure 316L stainless steel manifolded heat exchanger set with 8 coils. The tank is to be manufactured out of reinforced polyurethane panels. The panels are constructed from a 36kg/m³ polyurethane, foamed between 2 chromadek sheets. Rated to an R-value of 2.65. Tank to be fitted with 36 kW of immersion resistance heating elements for back-up heating.","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Heat exchanger coil (Stainless steel SU-316L, 10 Bar working pressure, 3l/s flow rate, 15°C to 65°C and 50mm primary and secondary water connections) for heat accumulator T-03.","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Preheating Tanks","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Heat accumulator c/w tank float valve, filling station, 3 sensor pockets, insulation and cladding and 36 kW electrical resistance elements. Refer to Part C3.3 Hot water storage tanks","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Heat accumulator, 11m³, T-03, low pressure thermal hot water tank, incorporating a high pressure 316L stainless steel manifolded heat exchanger set. The tank is to be manufactured out of reinforced polyurethane panels. The panels are constructed from a 36kg/m³ polyurethane, foamed between 2 chromadek sheets. Rated to an R-value of 2.65. Tank to be fitted with 36 kW of immersion resistance heating elements for back-up heating","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Heat exchanger coil (Stainless steel SU-316L, 10 Bar working pressure, 3l/s flow rate, 15°C to 65°C and 50mm primary water connections with 100mm secondary connections for chiller desuperheater piping) for heat accumulator T-03","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Domestic water pumps ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Water pump set c/w control panel anti-vibration mounting pads, frame chemical anchored on concrete plinth. Refer to Part C3.3 Pumps","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["3set Water pump set, 30ℓ/s, 600kPa, 2N+1,  5kW Motor each, P - 01 (2 duty 1 standby) including control panel as per technical specification. (One pump set has 3 pumps)","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over for pumps and pump sets","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Bladder type expansion vessel/ Diaphragm tank to suit pump and/or pump set  c/w 50mm braided hose connection and fittings","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["CiM Communication Module for BMS connection to Modbus and BACnet Inclusive of installatoin and all wiring","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D9309*C9309","v":{"v":0,"d":"R0.00"}}]
["Dry-run protection per pumpset through high and low level float switches installed inside the domestic water storage tanks","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Heat pump circulation pumps  ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Water pumps c/w anti-vibration mounting pads (Hot water circulating pumps between heat pump and heat accumulator). Refer to Part C3.3 Pumps","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Hot water circulation pump, Ø32mm, 1.4ℓ/s, 90kPa each, P - 03","No",10,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over for pumps and pump sets","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Motor protection per pump c/w pump guard control panel and fittings, wiring by others . IP54 Pump motor protection control panel with display for two pumps c/w motor protection for under voltage, over voltage, over load, dry run protection - sensor free, pump stalling and repeat start with RS485 comms interface, passive dry contact for fault signal and pipe temperature sensor function. Single phase for direct on line pumps, wiring by others. Pump guard or equal and approved by the wet services engineer.","No",10,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Building main circulating pumps ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Water pumps c/w anti-vibration mounting pads (Hot water circulating pumps between building and hot water plant). Refer to Part C3.3 Pumps","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Hot water circulation pump, Ø32mm, 2ℓ/s, 390kPa each, P - 02","No",10,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over for pumps and pump sets","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Motor protection per pump c/w pump guard control panel and fittings, wiring by others . IP54 Pump motor protection control panel with display for two pumps c/w motor protection for under voltage, over voltage, over load, dry run protection - sensor free, pump stalling and repeat start with RS485 comms interface, passive dry contact for fault signal and pipe temperature sensor function. Single phase for direct on line pumps, wiring by others. Pump guard or equal and approved by the wet services engineer.","No",10,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Preheating circulating pumps ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Water pumps c/w anti-vibration mounting pads (Hot water circulating pumps between building and hot water plant). Refer to Part C3.3 Pumps","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Hot water circulation pump, Ø80mm, 4ℓ/s, 90kPa each, P - 04","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over for pumps and pump sets","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Motor protection per pump c/w pump guard control panel and fittings, wiring by others . IP54 Pump motor protection control panel with display for two pumps c/w motor protection for under voltage, over voltage, over load, dry run protection - sensor free, pump stalling and repeat start with RS485 comms interface, passive dry contact for fault signal and pipe temperature sensor function. Single phase for direct on line pumps, wiring by others. Pump guard or equal and approved by the wet services engineer.","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Building branch circulating pumps ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Water pumps c/w anti-vibration mounting pads (Hot water circulating pumps between building and hot water plant). Refer to Part C3.3 Pumps","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Hot water circulation pump, Ø32mm, 1ℓ/s, 90kPa each, P - 02","No",34,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over for pumps and pump sets","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Motor protection per pump c/w pump guard control panel and fittings, wiring by others . IP54 Pump motor protection control panel with display for two pumps c/w motor protection for under voltage, over voltage, over load, dry run protection - sensor free, pump stalling and repeat start with RS485 comms interface, passive dry contact for fault signal and pipe temperature sensor function. Single phase for direct on line pumps, wiring by others. Pump guard or equal and approved by the wet services engineer.","No",34,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["FIRE EQUIPMENT, ETC ON WALL MOUNTED HANGERS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fire hose reel to SABS 543 complete with 580mm diameter hose reel, 20mm diameter rubber hose 30m long, 25mm diameter ,25mm diameter ball valve, 3000 chromium plated stopcock, shut-off nozzle and wall bracket","No",252,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["2.5kg Water Chemical fire extinguisher including hanger fixed to and including timber backing board.","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["4.5kg Dry chemical powder fire extinguisher including hanger fixed to and including timber backing board.","No",614,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["9kg Dry chemical powder fire extinguisher including hanger fixed to and including timber backing board.","No",10,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["2kg CO2 fire extinguisher including hanger fixed to and including timber backing board.","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["5kg CO2 fire extinguisher including hanger fixed to and including timber backing board.","No",15,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["WATER SUPPLIES TO FIRE APPLIANCES","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Galvanised steel pipes","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["25mm Pipes fixed walls with M10 rubber lined hanger brackets including M10 threaded rod not exceeding 500mm long and M10 drop-in anchor","m",1028,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["32mm Pipes fixed walls with M10 rubber lined hanger brackets including M10 threaded rod not exceeding 500mm long and M10 drop-in anchor","m",16,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D9373*C9373","v":{"v":0,"d":"R0.00"}}]
["80mm Pipes fixed walls with M10 rubber lined hanger brackets including M10 threaded rod not exceeding 500mm long and M10 drop-in anchor","m",32,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100mm Pipes fixed walls with M10 rubber lined hanger brackets including M10 threaded rod not exceeding 500mm long and M10 drop-in anchor","m",1156,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150mm Pipes fixed walls with M10 rubber lined hanger brackets including M10 threaded rod not exceeding 500mm long and M10 drop-in anchor","m",220,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["25mm Pipes fixed in suspended ceilings with M10 rubber lined hanger brackets including M10 threaded rod not exceeding 500mm long and M10 drop-in anchor","m",1337,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["32mm Pipes fixed in suspended ceilings with M10 rubber lined hanger brackets including M10 threaded rod not exceeding 500mm long and M10 drop-in anchor","m",249,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["40mm Pipes fixed in suspended ceilings with M10 rubber lined hanger brackets including M10 threaded rod not exceeding 500mm long and M10 drop-in anchor","m",37,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["50mm Pipes fixed in suspended ceilings with M10 rubber lined hanger brackets including M10 threaded rod not exceeding 500mm long and M10 drop-in anchor","m",29,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["65mm Pipes fixed in suspended ceilings with M10 rubber lined hanger brackets including M10 threaded rod not exceeding 500mm long and M10 drop-in anchor","m",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["80mm Pipes fixed in suspended ceilings with M10 rubber lined hanger brackets including M10 threaded rod not exceeding 500mm long and M10 drop-in anchor","m",115,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100mm Pipes fixed in suspended ceilings with M10 rubber lined hanger brackets including M10 threaded rod not exceeding 500mm long and M10 drop-in anchor","m",1555,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150mm Pipes fixed in suspended ceilings with M10 rubber lined hanger brackets including M10 threaded rod not exceeding 500mm long and M10 drop-in anchor","m",2065,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["200mm Pipes fixed in suspended ceilings with M10 rubber lined hanger brackets including M10 threaded rod not exceeding 500mm long and M10 drop-in anchor","m",496,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over galvanised steel pipes for steel fittings","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["25mm Bend","No",166,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["25mm Pressure reducing valve","No",252,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["25mm Tee","No",9,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["32mm Bend","No",18,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["32 x 25mm Reducing socket","No",24,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["32mm Tee","No",13,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["40mm Bend","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["40 x 25mm Reducing socket","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["40 x 40 x 25mm Reducing tee","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["50mm Bend","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["50mm Tee","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["50 x 50 x 25mm Reducing tee","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["50 x 32mm Reducing socket","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["50 x 40mm Reducing socket","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["65mm Bend","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["65 x 40mm Reducing socket ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["65 x 65 x 25mm Reducing tee","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["80mm Bend","No",18,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["80mm Tee","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D9437*C9437","v":{"v":0,"d":"R0.00"}}]
["80 x 80 x 25mm Reducing tee","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["80 x 50 x 32mm Reducing tee","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100mm Bend","No",216,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100mm Tee","No",10,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100 x 25mm Reducing socket ","No",7,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100 x 50mm Reducing socket ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100 x 80mm Reducing socket","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100 x 100 x 25mm Reducing tee","No",133,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100 x 100 x 32mm Reducing tee","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100 x 100 x 80mm Reducing tee","No",176,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150mm Bend ","No",125,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150mm Tee","No",34,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150 x 25mm Reducing socket ","No",8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150 x 80mm Reducing socket ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150 x 100mm Reducing socket ","No",54,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150 x 150 x 25mm Reducing tee","No",41,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150 x 150 x 32mm Reducing tee","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150 x 150 x 40mm Reducing tee","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150 x 150 x 80mm Reducing tee","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150 x 150 x 100mm Reducing tee","No",31,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["200mm Bend","No",8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["200mm Tee","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["200 x 150mm Reducing socket ","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["200 x 200 x 150mm Reducing tee","No",14,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Taps, Valves, etc.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["80mm Diameter Right angle type shielded spindle hydrant valve with 65mm threaded inlet","No",176,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150mm Isolating valve ","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TESTING","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Pressure testing fire pipe system","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["HOLES ETC","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Core drilling hole not exceeding 50mm diameter","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["300mm Concrete slab","No",134,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D9501*C9501","v":{"v":0,"d":"R0.00"}}]
["Core drilling hole exceeding 50mm and not exceeding 100mm diameter","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["300mm Concrete slab","No",114,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Core drilling hole exceeding 100mm and not exceeding 200mm diameter","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["300mm Concrete slab","No",283,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TOTAL INTERNAL PLUMBING AND DRAINAGE ",null,0,null,{"$f":"SUM(E8421:E9509)","v":{"v":0,"d":"0.00"}}]
[null,null,0,null,{"v":0,"d":"R0.00"}]
["SECTION 2","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NEW HOSPITAL ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["BILL NO 15","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["GLAZING","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PREAMBLES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Preambles for Trades as defined in Scope of Work (C3.1 Item 4.1 & Item 4.2)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TRADE NAMES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["No reference to trade names shall be made in these Bills of Quantities. Any reference to trade names in the Architect's specification or drawings shall deem to mean \"or similar and approved\"",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 150 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["GLAZING TO ALUMINIUM FRAMES (FRAMES ELSEWHERE)","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["6.38mm Clear intruder proof safety glass","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Panes exceeding 0,1m2 and not exceeding 0,5m2","m2",120,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PANELS, MIRRORS, ETC.","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["6mm Silvered float glass copper backed mirrors with bevelled edges holed for and fixed with chromium plated dome capped mirror screws with rubber buffers to plugs in brickwork or concrete","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Mirror 450 x 600mm high with bevelled edges. Plugged and screwed to tiled walls with four chromed mirror screws with dome caps ","No",862,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Mirror 450 x 900mm high with bevelled edges. Plugged and screwed to tiled walls with four chromed mirror screws with dome caps ","No",183,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Mirror 600 x 1800mm high with bevelled edges. Plugged and screwed to tiled walls with four chromed mirror screws with dome caps ","No",10,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["6mm Silvered PVB laminated safety glass copper backed mirrors with bevelled edges holed for and fixed with chromium plated dome capped mirror screws with rubber buffers to plugs in brickwork or concrete","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Mirror 450 x 900mm high with bevelled edges. Plugged and screwed to tiled walls with four chromed mirror screws with dome caps ","No",89,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke mirrors, concealed thief resistant fixings, plugged and screwed to the wall with stainless steel screws or similar approved. ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 500 x 900mm (Purpose made) M600HD 8mm mirrors, concealed thief resistant fixings, plugged and screwed to the wall with stainless steel screws. ","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Franke 500 x 600 model MH600R Chronos reflective polished surface mirror with concealed fixings Installed strictly to manufacturers specifications","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TOTAL GLAZING ",null,0,null,{"$f":"SUM(E9511:E9555)","v":{"v":0,"d":"0.00"}}]
[null,null,0,null,{"v":0,"d":"R0.00"}]
["SECTION 2","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NEW HOSPITAL ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["BILL NO 16","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PAINTWORK","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D9565*C9565","v":{"v":0,"d":"R0.00"}}]
["PREAMBLES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Preambles for Trades as defined in Scope of Work (C3.1 Item 4.1 & Item 4.2)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TRADE NAMES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Any reference to trade names in the Bills of Quantities or  Architect's specification or drawings shall deem to mean \"or similar and approved\"",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 152 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["ON FLOATED PLASTER","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Prepare surfaces and remove all loose material and rinse.  Surfaces to be dry, sound and clean and cured for stipulated 28 or 14 days as stated with a moisture content, measured with a Doser Hygrometer of BD 2 scale - 8%.  Apply with one coat unreduced 100% pure acrylic emulsion water based Versus primer with two coats 100% pure acrylic water based Versus Versatex paint enhanced with marble aggregate, fillers and fungicides or similar approved.  All to manufacturer’s detailed specifications. TVOC limits (g/L of product) to be compliant to TVOC limits in Table IEQ13.1 for Green Star PEB - Custom Healthcare. Colour to Architect’s selection (Ref. C3) ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On internal walls","m2",127535,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On columns","m2",239,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On beams","m2",43,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Prepare surfaces and remove all loose material and rinse.  Surfaces to be dry, sound and clean and cured for stipulated 28 or 14 days as stated with a moisture content, measured with a Doser Hygrometer of BD 2 scale - 8%.  Apply with one coat unreduced 100% pure acrylic emulsion water based Versus primer with two coats 100% pure acrylic water based Versus Aqua Ripple paint enhanced with marble aggregate, fillers and fungicides or similar approved.  All to manufacturer’s detailed specifications. TVOC limits (g/L of product) to be compliant to TVOC limits in Table IEQ13.1 for Green Star PEB - Custom Healthcare. Colour to Architect’s selection (Ref. C5)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On internal walls","m2",37870,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On external walls","m2",5499,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Prepare surfaces and remove all loose material and rinse.  Surfaces to be dry, sound and clean and cured for stipulated 28 or 14 days as stated with a moisture content, measured with a Doser Hygrometer of BD 2 scale - 8%.  Apply with one coat unreduced 100% pure acrylic emulsion water based Versus primer with two coats 100% pure acrylic water based Versus Texture paint enhanced with marble aggregate, fillers and fungicides or similar approved. All to manufacturer’s detailed specifications. TVOC limits (g/L of product) to be compliant to TVOC limits in Table IEQ13.1 for Green Star PEB - Custom Healthcare. Colour to Architect’s selection (Ref. H14)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On external walls","m2",4548,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Prepare surfaces and remove all loose material and rinse.  Surfaces to be dry, sound and clean and cured for stipulated 28 or 14 days as stated with a moisture content, measured with a Doser Hygrometer of BD 2 scale - 8%.  Apply with one coat unreduced 100% pure acrylic emulsion water based Versus primer with two coats 100% pure acrylic water based Versus Surewall paint enhanced with marble aggregate, fillers and fungicides or similar approved.  All to manufacturer’s detailed specifications. TVOC limits (g/L of product) to be compliant to TVOC limits in Table IEQ13.1 for Green Star PEB - Custom Healthcare. Colour to Architect’s selection (Ref. H38)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On external walls","m2",45551,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On external beams","m2",27147,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On external columns ","m2",3557,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Prepare surfaces and remove all loose material and rinse.  Surfaces to be dry, sound and clean and cured for stipulated 28 or 14 days as stated with a moisture content, measured with a Doser Hygrometer of BD 2 scale - 8%.  Apply with one coat unreduced 100% pure acrylic emulsion water based Versus primer with two coats 100% pure acrylic water based Versus Tershan Trowel paint enhanced with marble aggregate, fillers and fungicides or similar approved.  All to manufacturer’s detailed specifications. TVOC limits (g/L of product) to be compliant to TVOC limits in Table IEQ13.1 for Green Star PEB - Custom Healthcare. Colour to Architect’s selection (Ref. H65)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On external walls","m2",3589,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Prepare surfaces and remove all loose material and rinse.  Surfaces to be dry, sound and clean and cured for stipulated 28 or 14 days as stated with a moisture content, measured with a Doser Hygrometer of BD 2 scale - 8%.  Apply with one coat unreduced 100% pure acrylic emulsion water based Versus primer with two to three coats 100% pure acrylic water based Versus Natural Stone paint (sprayed on) enhanced with natural stone marble quarts and fungicides or similar approved. All to manufacturer’s detailed specifications. TVOC limits (g/L of product) to be compliant to TVOC limits in Table IEQ13.1 for Green Star PEB - Custom Healthcare. Colour to Architect’s selection (Ref. H230)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On external walls","m2",3591,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Prepare surfaces and remove all loose material and rinse.  Surfaces to be dry, sound and clean and cured for stipulated 28 or 14 days as stated with a moisture content, measured with a Doser Hygrometer of BD 2 scale - 8%.  Apply with one coat unreduced 100% pure acrylic emulsion water based Versus primer with one coat 100% pure acrylic water based Versus Comb Plaster paint enhanced with marble quarts fillers and fungicides or similar approved. All to manufacturer’s detailed specifications. TVOC limits (g/L of product) to be compliant to TVOC limits in Table IEQ13.1 for Green Star PEB - Custom Healthcare. Colour to Architect’s selection (Ref. H239)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On external walls","m2",3591,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Prepare surfaces and remove all loose material and rinse.  Surfaces to be dry, sound and clean and cured for stipulated 28 or 14 days as stated with a moisture content, measured with a Doser Hygrometer of BD 2 scale - 8%.  Apply with one coat unreduced 100% pure acrylic emulsion water based Versus primer with one coat 100% pure acrylic water based Versus Italic Plaster paint enhanced with marble quarts fillers and fungicides or similar approved. All to manufacturer’s detailed specifications. TVOC limits (g/L of product) to be compliant to TVOC limits in Table IEQ13.1 for Green Star PEB - Custom Healthcare. Colour to Architect’s selection (Ref. H277)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On external walls","m2",3589,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Prepare surfaces and remove all loose material and rinse.  Surface to be dry, sound and clean and cured for a minimum of 28 days, with a moisture content, measured with a Doser Hygrometer of BD 4 scale - 5% or less.  Prime with one coat Versus plaster primer with an over coating time of 16 hours and finish with two coats Versus status Matt with 2 hours drying time between coats or similar approved. All to manufacturer’s detail specifications. TVOC limits (g/L of product) to be compliant to TVOC limits in Table IEQ13.1 for Green Star PEB - Custom Healthcare. Colour to Architect’s approval","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On plastered ceilings","m2",11083,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["ON FIBRE CEMENT","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Prepare surfaces and remove all loose material. Prime with one coat of Versus Universal Undercoat with an overcoating time of 16 hours and finish with one coat of Versus Status Matt acrylic paint thinned 20% and one coat of Versus Status Matt acrylic paint or similar approved. All to manufacturer’s detail specifications. TVOC limits (g/L of product) to be compliant to TVOC limits in Table IEQ13.1 for Green Star PEB - Custom Healthcare. Colour to Architect’s approval","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On fibre cement ceilings","m2",6797,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D9629*C9629","v":{"v":0,"d":"R0.00"}}]
["ON PLASTER BOARD","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Prepare surfaces and remove all loose material.  Apply with one coat unreduced 100% pure acrylic emulsion water based Versus primer with two coats 100% pure acrylic water based Versus Versatex paint enhanced with marble aggregate, fillers and fungicides or similar approved.  All to manufacturer’s detailed specifications. TVOC limits (g/L of product) to be compliant to TVOC limits in Table IEQ13.1 for Green Star PEB - Custom Healthcare. Colour to Architect’s selection (Ref. C3)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On partitioning ","m2",8028,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Prepare surfaces and remove all loose material.  Apply with one coat unreduced 100% pure acrylic emulsion water based Versus primer with two coats 100% pure acrylic water based Versus Aqua Ripple paint enhanced with marble aggregate, fillers and fungicides or similar approved. All to manufacturer’s detailed specifications. TVOC limits (g/L of product) to be compliant to TVOC limits in Table IEQ13.1 for Green Star PEB - Custom Healthcare. Colour to Architect’s selection (Ref. C5)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On partitioning ","m2",2341,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Prepare surfaces and remove all loose material. Prime with one coat of Versus Universal Undercoat with an overcoating time of 16 hours and finish with one coat of Versus Status Matt acrylic paint thinned 20% and one coat of Versus Status Matt acrylic paint or similar approved. All to manufacturer’s detail specifications. TVOC limits (g/L of product) to be compliant to TVOC limits in Table IEQ13.1 for Green Star PEB - Custom Healthcare. Colour to Architect’s approval","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On plasterboard ceilings","m2",3347,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On bulkheads","m2",1511,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["ON FACED BRICKWORK","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Prepare surfaces and remove all loose material and finish with Chryso Drikote Sealer or similar approved. All to manufacturer’s detail specifications. TVOC limits (g/L of product) to be compliant to TVOC limits in Table IEQ13.1 for Green Star PEB - Custom Healthcare. Colour to Architect’s approval (C15)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Walls","m2",618,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["ON METALWORK","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Prepare frame and apply Plascon Galvanised Iron Cleaner (GIC1) to all bare galvanised areas, allow to react for one minute and rinse off with tap water using bristle brush or Scotch Brite pads. Prime with one coat of Galvanised Iron Primer (GIP1) with an overcoating time of 24 hours and finish with two coats of Velvaglo Satin (VLO) with 16 hours drying time between coats or similar approved. TVOC limits (g/L of product) to be compliant to TVOC limits in Table IEQ13.1 for Green Star PEB - Custom Healthcare. Colour to Architects approval","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On door frames","m2",6984,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On record room doors ","m2",73,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Prepare frame and apply one coat Plascoguard 75 Zinc Phosphate Epoxy Primer (PEX75/PEH75) with an overcoating tim of 4 hours finish with two coats Plascothane Polyurethane Enamel (UP1) with 30 minutes drying time between coats or similar approved. TVOC limits (g/L of product) to be compliant to TVOC limits in Table IEQ13.1 for Green Star PEB - Custom Healthcare. Colour to Architects approval.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On window mullions, etc.","m2",38,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On steel menbers (Provisional) ","m2",120,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On steel not exceeding 300mm girth","m",1361,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Apply Plascon Galvanised Iron Cleaner (GIC 1) to all bare galvanised areas. Allow to react for 1 minute and rinse off with tap water using bristle brush or Scotch Brite pads to remove all surface contaminants, until surface is water break-free. Prime with one coat of Galvanised Iron Primer (GIP 1) with an overcoating time of 24 hours and finish with two coats of Velvaglo Satin (VLO) with 16 hours drying time between coats, for a maintenance cycle of 3 years or similar approved. TVOC limits (g/L of product) to be compliant to TVOC limits in Table IEQ13.1 for Green Star PEB - Custom Healthcare. Colours to Architect’s approval.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fire water pipes","m2",510,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fire water pipes not exceeding 300mm girth","m",536,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["ON WOOD","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Stop, fill, sand down and prepare wood surface. Wash knots and resinous areas with lacquer thinners and coat with Woodcare Knot Seal (PK2), apply one coat of Plascon Woodcare Pretreatment (WWP1) overcoated within 48 hours, prime with one coat of Wood Primer (UC2) with an overcoating time of 16 hours and finish with two coats of Velvaglo Satin (VLO) with 16 hours drying time between coats or similar approved. All to manufacturer’s detail specifications. TVOC limits (g/L of product) to be compliant to TVOC limits in Table IEQ13.1 for Green Star PEB - Custom Healthcare.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On doors","m2",15202,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Stop, fill, sand down and prepare wood surface. One coat wood primer one undercoat and two coats oil based (Versus Matt Enamel) paint system or similar approved. TVOC limits (g/L of product) to be compliant to TVOC limits in Table IEQ13.1 for Green Star PEB - Custom Healthcare.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On skirting, rails, bars, etc. not exceeding 300mm girth","m",1865,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TOTAL PAINTWORK ",null,0,null,{"$f":"SUM(E9557:E9683)","v":{"v":0,"d":"0.00"}}]
[null,null,0,null,{"v":0,"d":"R0.00"}]
["SECTION 2","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NEW HOSPITAL ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["BILL NO 17","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["BUILDERS WORK (PROVISIONAL) ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D9693*C9693","v":{"v":0,"d":"R0.00"}}]
["PREAMBLES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Preambles for Trades as defined in Scope of Work (C3.1 Item 4.1 & Item 4.2)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TRADE NAMES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Any reference to trade names in the Bills of Quantities or  Architect's specification or drawings shall deem to mean \"or similar and approved\"",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The Tenderer is referred to Section 2 and the JBCC CPAP work groups for similar items, which will apply equally to the work in this Bill unless otherwise described.",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE:All sleeve pipes and pipe conduits to be supplied with draw wires as necessary for fixing of cables and wiring",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 104 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["EXCAVATIONS, ETC.","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavate in earth and set excavated material aside for re-use as filling for:","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cable or sleeve trenches not exceeding 1m deep","m3",536,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over excavations in 'earth' for cable or sleeve trenches in 'intermediate rock'","m3",107,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over excavations in 'earth' for cable or sleeve trenches in 'hard rock'","m3",54,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Provide bedding from carted on material from commercial sources including sifting and compaction to 90% MOD AASHTO density for backfilling to","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Selected granular material","m3",94,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fill blanket from carted on material from commercial sources including sifting and compaction to 90% MOD AASHTO density for backfilling to","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Selected fill material","m3",189,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over all excavations for carting away","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Surplus material from excavations and/or stock piles on site to a dumping site to be located by the contractor","m3",300,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Risk of collapse of excavations","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sides of trench and hole excavations not exceeding 1,5m deep","m2",1258,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Keeping excavations free of water","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Keeping excavations free of water ","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Selected earth filling obtained from the excavations and/or prescribed stockpiles on site in layers of 150mm thick compacted to 93% Mod AASHTO density","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Backfilling to trenches, holes, etc.","m3",253,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["HOLES ETC","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Core drilling hole not exceeding 50mm diameter","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["220mm Brick wall","No",1461,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["300mm Concrete slab","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Core drilling hole exceeding 50mm and not exceeding 100mm diameter","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["220mm Brick wall","No",19,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["300mm Concrete slab","No",25,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Core drilling hole exceeding 100mm and not exceeding 200mm diameter","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D9757*C9757","v":{"v":0,"d":"R0.00"}}]
["220mm Brick wall","No",153,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["300mm Concrete slab","No",209,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 110 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["CONCRETE PLINTHS ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["REINFORCED CONCRETE","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["25MPa/19mm concrete","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Concrete plinths ","m3",65,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Finishing top surfaces of concrete smooth with a steel float","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Concrete plinths","m2",431,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 111 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Smooth formwork to sides","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["To sides of concrete plinths ","m2",211,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["To sides of concrete plinths not exceeding 300mm high ","m",431,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Boxing in rough formwork to form:","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["25 x 25mm Horizontal chamfer along corner of concrete plinth","m",783,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 114 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Mild steel rod reinforcement to structural concrete ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["8mm Diameter bars","t",1.05,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["High tensile steel rod reinforcement to structural concrete ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["10mm Diameter bars","t",1.05,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["12mm Diameter bars","t",1.05,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["16mm Diameter bars","t",1.05,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["20mm Diameter bars","t",1.05,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 116 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Openings through brickwork","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["300 x 300mm Opening through 220mm wall including necessary lintels ","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["500 x 400mm Opening through 220mm wall including necessary lintels ","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["500 x 500mm Opening through 220mm wall including necessary lintels ","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 146 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SLEEVES ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["uPVC sleeves laid in trenches (trenches elsewhere)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110mm Diameter sleeve pipes","m",580,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D9821*C9821","v":{"v":0,"d":"R0.00"}}]
["160mm Diameter sleeve pipes","m",165,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["uPVC sleeves laid in slabs","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["50mm Diameter sleeve pipes","m",805,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["75mm Diameter sleeve pipes","m",665,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110mm Diameter sleeve pipes","m",1612,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["MANHOLES","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Manhole formed of precast concrete rings of dolomite origin bedded and jointed with joints between rings sealed on the external perimeter with an approved high grade highly conformable cold applied corrosion protection petroleum tape, with bottom ring set on and including minimum 250mm thick concrete 20MPa slab (foundation) projecting beyond external face of manhole ring and sealed to ring with 20MPa concrete triangular fillet complete with and including 150mm thick 20MPa precast concrete cover slab to SABS 1294 specification with 750mm diameter shaft opening placed over precast concrete rings and bedded and jointed in polyamide cured thixotropic epoxy adhesive paste and with two 75mm thick precast reinforced concrete spacer slabs with 560mm diameter shaft opening placed over cover slab and bedded and jointed in polyamide cured thixotropic epoxy adhesive paste complete with and including galvanised malleable cast iron steps at 250mm vertical centres, including concrete 20MPa benching in bottom with top surfaces to falls and finished smooth with 3:1 mortar (plaster) coat complete with and including 150mm vitrified clay channels, channel beds, channel junctions, etc. including additional excavation and backfilling compacted to 90% Mod AASHTO","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Manhole 1000mm internal diameter not exceeding 1m deep","No",54,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Manhole 1000mm internal diameter not exceeding 1m deep","No",90,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Manhole 1500mm internal diameter not exceeding 1m deep","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PENETRATIONS IN ROOF SLABS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["All smooth formwork must be cleaned, all unevenness removed, properly prepared and then finished with a final coat of cementitious paint to give a smooth and even finish",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 111 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Smooth formwork to form","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Edges, risers, ends and reveals exceeding 300mm high or wide","m2",42,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Edges, risers, ends and reveals not exceeding 300mm high or wide","m",450,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Opening not exceeding 1m girth through not exceeding 300mm slab","No",75,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["AUDITORIUM ACOUSTIC INSTALLATION ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Provide the sum of R200 000.00 (Two Hundred Thousand Rand) nett for Auditorium Acoustic Installation","Item",1,{"v":200000,"d":"R200,000.00"},{"v":200000,"d":"R200,000.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for profit if required ","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for attendance","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["THE FOLLOWING IN STUDENT OBSERVATION ROOMS ","H1",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 104 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["EXCAVATION, FILLING, ETC","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavation in earth or compacted filling not exceeding 2m deep","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Holes","m3",72,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over excavations in earth for excavation in","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Soft rock","m3",8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Hard rock","m3",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over all excavations for carting away","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Surplus material from excavations and/or stock piles on site to a dumping site to be located by the contractor","m3",24,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Risk of collapse of excavations","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D9885*C9885","v":{"v":0,"d":"R0.00"}}]
["Sides of trench and holes exceeding 1,5m deep and not exceeding 3m deep","m2",192,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Selected earth filling obtained from the excavations and/or prescribed stock piles on site in layers of 150mm thick compacted to 93% Mod AASHTO density","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Backfilling to trenches, holes, etc","m3",48,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Approved G5 filling supplied and carted on by the Contractor, compacted in layers not exceeding 150mm to 95% Mod. AASHTO density","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Backfilling to trenches, holes, etc ","m3",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Soil insecticide in accordance with SANS 5859","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["To bottoms and sides of trenches and holes (Certificate to be supplied before payment is made)","m2",228,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 110 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["UNREINFORCED CONCRETE CAST AGAINST EXCAVATED SURFACES ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["15MPa/19mm concrete","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blinding under column bases","m3",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["REINFORCED CONCRETE CAST AGAINST EXCAVATED SURFACES ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["30 MPa/19 mm concrete in","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Column bases","m3",16,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Walls","m3",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Slabs","m3",60,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["50MPa/19mm concrete","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Columns","m3",15,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 111 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["FORMWORK","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["ROUGH FORMWORK (DEGREE OF ACCURACY II)","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Rough formwork to sides","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Walls exceeding 3.5m and not exceeding 5m high","m2",61,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Rectangular columns not exceeding 3.5m high","m2",28,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Rectangular columns exceeding 3.5m and not exceeding 5m high","m2",81,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Rough formwork to soffits of:","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Slabs exceeding 250mm and not exceeding 500mm thick, propping exceeding 3,5m and not exceeding 5m high","m2",200,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 114 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["REINFORCEMENT","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Mild steel rod reinforcement to structural concrete ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["8mm Diameter bars","t",3.58,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["High tensile steel rod reinforcement to structural concrete ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D9949*C9949","v":{"v":0,"d":"R0.00"}}]
["10mm Diameter bars","t",5.37,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["12mm Diameter bars","t",2.69,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["16mm Diameter bars","t",6.28,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 116 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SUPERSTRUCTURE","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Brickwork of clay bricks in 6:1 cement mortar","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["One brick walls","m2",76,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Brick reinforcement ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150mm Wide reinforcement built in horizontally ","m",223,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Prestressed concrete lintels","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["115mm Wide lintel in lengths not exceeding 3m","m",16,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 110 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["WATERPROOFING TO FLAT ROOFS ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sikalastic®-560 waterproofing membrane installed in accordance with the manufacturer`s specifications. (Sika 051 430 0333) or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On flat roofs to falls","m2",39,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Vertically to concrete upstand ","m2",13,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Horizontally to top of concrete upstand ","m2",8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["50mm Triangular fillet ","m",52,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 124 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PROFILED METAL SHEETING AND ACCESSORIES ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["0.53mm thick Global Roofing Solutions 700mm cover Klip-Tite™ profile Colorbond® Ultra Steel AZ200 spleter colour coated finish to top side - Colour: (Non standard colour to Architect's approval) and (Non standard colour to Architect's approval) backing coat roof sheeting, fixed to steel intermediate purlins at Max 2300mm centres and eaves and ridge purlins at Max 1900mm centres using KL700 clips, U-spacers to suit and sheet metal bearing strips of 150mm x 0.8mm thick over insulation fixed with 10No.16 x 16mm long self drilling wafer head PH2 screws or similar approved. All in accordance with the manufacturer`s specifications.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Roof sheeting with pitch not exceeding 25 degrees, fixed to steel purlins fixed concurrent with 40mm lambdaboard (measured elsewhere) ","m2",110,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Side cladding, fixed to steel purlins with additional screws to cladding rails fixed concurrent with 40mm lambdaboard (measured elsewhere) ","m2",116,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["40mm Lambdaboard density 34kg/m³ closed cell Polyisocyanurate insulation with White mineral facing to one side, fixed concurrent with roof covering over purlins with aluminium T section fixed at 1200mm centres or similar approved. All in accordance with the manufacturer's recommendations, complete with SABISA certificate.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Insulation laid over purlins fixed concurrent with roof covering ","m2",98,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["40mm Lambdaboard density 34kg/m³ laminated Polyisocyanurate with White mineral facing on one side and mineral natural on the other, fixed to the vertical frame work of the purlins. System to be mechanically fastened as per manufacturer’s instruction or similar approved. All in accordance with the manufacturer's recommendations, complete with SABISA certificate.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Insulation laid vertical over cladding rails fixed concurrent with side cladding ","m2",116,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 126 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["DOORS, ETC.","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["44mm Weatherboard flush door with vertical tongue and groove hardwood back to back boarding on both sides","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Single door size 813 x 2038mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["40mm Solid core flush panel door with masonite finish both sides with hardwood concealed edge strip fitted with lock block to one edge","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D10013*C10013","v":{"v":0,"d":"R0.00"}}]
["Double door 1436 x 2038mm high in two equal leaves","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["CUPBOARDS ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Supply and install Cupboards (PC Amount of R6000.00 per meter, excluding VAT). Rate to include manufacture, transportation, delivery and installation. ","m",8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PANELLING ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Supply and install Panelling, insulation (PC Amount of R950.00 per square meter, excluding VAT). Rate to include manufacture, transportation, delivery and installation. ","m2",116,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 129 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["INSULATION","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100mm Thick Isover Aerolite non-combustible light weight fibreglass Glasswool thermal ceiling insulation 12kg/m³ closely fitted with ends butted firmly between tie beams and laid loose on top of brandering between roof timbers or similar approved. All in accordance with manufacturer`s recommendations. (D69)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ceiling insulation","m2",102,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NAILED UP CEILINGS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Pelican Systems Jumbo Fibre Cement ceiling system with 6mm thick fibre cement board fixed at right angles to 38 x 38mm battens fixed to concrete at 600mm centres, using 25mm drywall screws at 150mm centres. All joints to be covered with a 6mm JUMBO Jointing Strip and prepared for decoration or similar approved. All in accordance with the manufacturer's instructions. (D3)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ceilings ","m2",102,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SUSPENDED PLASTERED GYPSUMBOARD CEILINGS AND BULKHEADS ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Pelican Systems JUMBO skimmed ceiling system with 9mm thick JUMBO plasterboard fixed at right angles using 25mm Jumbo drywall screws at 150mm centres to JUMBO steel brandering comprising JUMBO steel brandering at 400mm centres in one direction only. All joints to be covered with JUMBO fiba tape and the entire surface plastered with 3mm to 6mm thick JUMBO skimming plaster complete with SABISA certificate (D4) or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ceilings suspended not exceeding 1m below concrete soffits","m2",102,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Pelican Systems JUMBO skimmed ceiling system with 9mm thick JUMBO plasterboard fixed at right angles using 25mm Jumbo drywall screws at 150mm centres to JUMBO steel brandering comprising JUMBO steel brandering at 300mm centres in one direction only. All joints to be covered with JUMBO fiba tape and the entire surface plastered with 3mm to 6mm thick JUMBO skimming plaster complete with SABISA certificate (D15) or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sides of bulkheads, suspending exceeding 1m and not exceeding 2m below concrete","m2",20,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Soffits of  bulkheads, suspending not exceeding 1m below concrete","m2",24,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Pelican Systems Aluminium PS4 shadow wall trim, fixed to plastered brickwork with 5 x 25mm wall anchors at 450mm centres or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Shadowline cornice, fixed to walls","m",72,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 130 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["FLOOR COVERINGS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Polyflor 2mm thick Paletone PUR Homogeneous vinyl floor sheeting (colour to architects approval), laid in acrylic adhesive spread with a notched trowel on suitably prepared cement screed floors with a hygrometer reading showing a moisture content of less than 70%, with joints welded with a fully flexible coloured Polyflor welding rod to provide a smooth, hygienic sealed finish and rolled with 68kg articulated floor roller or similar approved. All in accordance with manufacturer`s recommendations. (A47)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Seamless vinyl floor sheets on floors","m2",108,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["200mm Wide border x  200mm high turn up against walls (400mm girth), including welding to floor covering (floor covering elsewhere) including all formed internal and external corners","m",81,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SKIRTINGS, NOSINGS, ETC","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cappings, cove formers, etc","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Polyflor Polycove cove former PC20 colour Black, size 20 x 20mm wide or similar approved. All in accordance with manufacturer`s specifications.","m",81,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Polyflor Clip-Top base CB30, size 29.5 x 5.4mm high, glue to wall with an approved adhesive or similar approved. All in accordance with manufacturer`s specifications.","m",81,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Polyflor Clip-Top capping CTC3 or similar approved. All in accordance with manufacturer`s specifications.","m",81,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 134 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["MILD STEEL","H1",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D10077*C10077","v":{"v":0,"d":"R0.00"}}]
["The following in welded and bolted roof trusses, erected approximately 8m above floor level ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Angle sections, flat sections, etc. in tie beams, rafters, struts, bracing, etc. of roof trusses","t",2.62,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["I sections, IPE sections, etc. in tie beams, rafters, struts, bracing, etc. of roof trusses","t",1.54,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Angle sections, flat sections, etc. in brackets, base plates,  connector plates, etc. ","t",0.34,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The following in welded and bolted steel columns and beams","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["I-section and H-section columns and beams","t",1.39,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Angle sections in bracing, etc.","t",0.38,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Angle sections, flat sections, etc. in brackets, base plates,  connector plates, etc.","t",0.08,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["FIRE ESCAPE STAIRCASE  ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow the amount of R150 000.00 (One Hundred and Fifty Thousand Rand) for the construction of fire escape staircase. This work will be measured on completion and priced at scheduled rates.","No",1,{"v":150000,"d":"R150,000.00"},{"v":150000,"d":"R150,000.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PLANTROOMS ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The following in welded and bolted steel columns and beams ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Vital Engineering Vitagrid pressure forged VE40Z modular walkway panel with 25 x 45mm serrated non-slip bearer bars in galvanised mild steel including banding on all sides or similar approved, laid in mild steel angle (elsewhere measured)","m2",87,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["I-section and H-section columns and beams","t",2.96,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Angle sections in bracing, etc.","t",0.89,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Angle sections, flat sections, etc. in brackets, base plates,  connector plates, etc.","t",0.18,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 136 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["HANDRAILS, BALUSTRADES.","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Supply and install Balustrading (PC Amount of R1500.00 per meter, excluding VAT). Rate to include manufacture, transportation, delivery and installation. ","m",32,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SEATING ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Supply and install Seating (PC Amount of R3500.00 per seat, excluding VAT). Rate to include manufacture, transportation, delivery and installation. ","No",63,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PRESSED STEEL DOOR FRAMES","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["1.2mm Double rebated frames suitable for one brick walls and fitted with one pair of screw on stainless steel ball bearing hinges per door leaf","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Frame for door 813 x 2038mm high ","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Frame for double door 1436 x 2038mm high ","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 140 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["ALUMINIUM WINDOWS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Purpose made standard colour polyester powder coated aluminium windows with glass panes and/or solid aluminium panels as stated, window furniture, screws and bolts installed complete strictly according to AAAMSA standards and specifications","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Supply and install Windows (PC Amount of R2500.00 per square meter, excluding VAT). Rate to include manufacture, transportation, delivery and installation. ","m2",15,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 142 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SCREEDS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["1:3 Cement plaster screeds on concrete","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D10141*C10141","v":{"v":0,"d":"R0.00"}}]
["30mm Thick on floors","m2",108,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Average 80mm Thick on concrete roofs to falls and currents ","m2",39,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SPECIALIST FLOOR COVERINGS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["3mm Thick \"Levelite\" or similar approved self-levelling screeds (approved and installed by flooring sub-contractor) on concrete surface beds to obtain a level surface and providing a quality base. Sub surface to be primed and dry (moisture test to be done) to ensure a quality and sound application,  all applied in strict accordance with the manufacturer's specifications, on: ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On floors ","m2",108,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["INTERNAL PLASTER","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["One coat 1:4 cement plaster on concrete with steel trowel and no other finish (Ref. C1) ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On walls","m2",194,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 152 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["ON FLOATED PLASTER","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Prepare surfaces and remove all loose material and rinse.  Surfaces to be dry, sound and clean and cured for stipulated 28 or 14 days as stated with a moisture content, measured with a Doser Hygrometer of BD 2 scale - 8%.  Apply with one coat unreduced 100% pure acrylic emulsion water based Versus primer with two coats 100% pure acrylic water based Versus Versatex paint enhanced with marble aggregate, fillers and fungicides or similar approved. All to manufacturer’s detailed specifications. TVOC limits (g/L of product) to be compliant to TVOC limits in Table IEQ13.1 for Green Star PEB - Custom Healthcare. Colour to Architect’s selection (Ref. C3) ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On internal walls","m2",194,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["ON FIBRE CEMENT","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Prepare surfaces and remove all loose material. Prime with one coat of Versus Universal Undercoat with an overcoating time of 16 hours and finish with one coat of Versus Status Matt acrylic paint thinned 20% and one coat of Versus Status Matt acrylic paint or similar approved. All to manufacturer’s detail specifications. TVOC limits (g/L of product) to be compliant to TVOC limits in Table IEQ13.1 for Green Star PEB - Custom Healthcare. Colour to Architect’s approval","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On fibre cement ceilings","m2",102,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["ON PLASTER BOARD","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Prepare surfaces and remove all loose material. Prime with one coat of Versus Universal Undercoat with an overcoating time of 16 hours and finish with one coat of Versus Status Matt acrylic paint thinned 20% and one coat of Versus Status Matt acrylic paint or similar approved. All to manufacturer’s detail specifications. TVOC limits (g/L of product) to be compliant to TVOC limits in Table IEQ13.1 for Green Star PEB - Custom Healthcare. Colour to Architect’s approval","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On plasterboard ceilings","m2",102,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On bulkheads","m2",44,null,{"v":0,"d":"R0.00"}]
[]
["TOTAL BUILDERS WORK IN CONNECTION WITH ELECTRICAL AND MECHANICAL SERVICES ",null,0,null,{"$f":"SUM(E9685:E10179)","v":{"v":350000,"d":"350,000.00"}}]
[null,null,0]
["Foundations (Provisional)",null,null,{"v":0,"d":"R0.00"},{"$f":"E1216","v":{"v":0,"d":"R0.00"}}]
[]
["Concrete, Formwork & Reinforcement ",null,null,{"v":0,"d":"R0.00"},{"$f":"E1532","v":{"v":0,"d":"R0.00"}}]
[]
["Masonry",null,null,{"v":0,"d":"R0.00"},{"$f":"E1702","v":{"v":0,"d":"R0.00"}}]
[]
["Waterproofing",null,null,{"v":0,"d":"R0.00"},{"$f":"E1790","v":{"v":0,"d":"R0.00"}}]
[]
["Roof Coverings etc",null,null,{"v":0,"d":"R0.00"},{"$f":"E1902","v":{"v":0,"d":"R0.00"}}]
[]
["Carpentry & Joinery",null,null,{"v":0,"d":"R0.00"},{"$f":"E2616","v":{"v":0,"d":"R0.00"}}]
[]
["Ceilings, Partitions & Access Flooring",null,null,{"v":0,"d":"R0.00"},{"$f":"E2910","v":{"v":100000,"d":"R100,000.00"}}]
[]
["Floor Coverings Plastic Linings etc",null,null,{"v":0,"d":"R0.00"},{"$f":"E3078","v":{"v":0,"d":"R0.00"}}]
[]
["Ironmongery ",null,null,{"v":0,"d":"R0.00"},{"$f":"E4914","v":{"v":0,"d":"R0.00"}}]
[]
["Structural Steelwork ",null,null,{"v":0,"d":"R0.00"},{"$f":"E5084","v":{"v":600000,"d":"R600,000.00"}}]
[]
["Metalwork",null,null,{"v":0,"d":"R0.00"},{"$f":"E8164","v":{"v":0,"d":"R0.00"}}]
[]
["Plastering",null,null,{"v":0,"d":"R0.00"},{"$f":"E8344","v":{"v":0,"d":"R0.00"}}]
[]
["Tiling",null,null,{"v":0,"d":"R0.00"},{"$f":"E8420","v":{"v":0,"d":"R0.00"}}]
[]
["Internal Plumbing & Drainage (Provisional)",null,null,{"v":0,"d":"R0.00"},{"$f":"E9510","v":{"v":0,"d":"R0.00"}}]
[]
["Glazing",null,null,{"v":0,"d":"R0.00"},{"$f":"E9556","v":{"v":0,"d":"R0.00"}}]
[]
["Paintwork",null,null,{"v":0,"d":"R0.00"},{"$f":"E9684","v":{"v":0,"d":"R0.00"}}]
[]
["Builderswork (Provisional) ",null,null,{"v":0,"d":"R0.00"},{"$f":"E10180","v":{"v":350000,"d":"R350,000.00"}}]
[]
["TOTAL SECTION 2 CARRIED TOFINAL SUMMARY",null,0,null,{"$f":"SUM(E10181:E10215)","v":{"v":1050000,"d":"1,050,000.00"}}]
[]
["SECTION 3","H2",0]
[]
["THERMAL ACTIVATED BUILDING SYSTEM (PROVISIONAL) ","H2",0]
[]
["BILL NO 1","H2",0]
[]
["THERMAL ACTIVATED BUILDING SYSTEM","H2",0]
[]
["PREAMBLES","H3",0]
[]
["Preambles for Trades as defined in Scope of Work (C3.1 Item 4.1 & Item 4.2)","H3",0]
[]
["TRADE NAMES","H3",0]
[]
["Any reference to trade names in the Bills of Quantities or  Architect's specification or drawings shall deem to mean \"or similar and approved\"",null,0]
[]
["NOTE: The following items shall be deemed to fall into Work Group No 148 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[]
["PREAMBLE:  PLEASE NOTE THAT THIS BOQ HAS TO BE READ IN CONJUNCTION WITH THE SPECIFICATION AND DRAWINGS.  THE MAIN CONTRACTOR SHALL ENSURE THAT THE SUB CONTRACTOR RECEIVE A COMPLETE COPY OF THE ABOVE DOCUMENTS.  IF THE ENGINEER DOES DUE DILIGENCE WHEN EVALUATING THE TENDER AND FIND THAT THE SUB CONTRACTORS DID NOT RECEIVE A COPY OF THE ABOVE DOCUMENTATION, THE PRICE WILL BE INVALID.",null,0]
[]
["Applicable Specifications:","H3",0]
[]
["T80 TABS","H3",0]
[]
["PART  1   GENERAL  T80 -1.1 Section includes A. Concrete Embedded Pipe System  T80 -1.2 References A. Building Engineering Services Association: TR/11: Guide To The Use Of Plastic Pipework. B. En 15377-2:2008: Heating Systems in Buildings — Design of Embedded Water Based Surface Heating And Cooling Systems — Part 2: Design, Dimensioning and Installation  T80 -1.3 Related Sections A. T61 – Primary / Secondary Cooling Solutions  T80 -1.4 Scope A. Supply, delivery and installation of TABS embedded piping. B. On site Rigging.  T80 -1.5 Submittals A. Manufacturer's data sheets on each product to be used. B. Preparation instructions and recommendations. C. Storage and handling requirements and recommendations. D. Typical installation methods.  T80 -1.6 Quality assurance A. Manufacturer Qualifications: Company specializing in manufacturing products specified in this section with a minimum five years documented experience. B. Installer Qualifications: Company specializing in performing work of this section with minimum two years documented experience with projects of similar scope and complexity. C. Source Limitations: Provide each type of product from a single manufacturing source to ensure uniformity.  T80 -1.5 12-Month Warranty And Maintenance A. All chilled water and TABS piping installations will be warranted for 12 months from date of commissioning, regardless of start-up date.",null,0]
[]
["PART 2 - PRODUCTST80 -2.1 PipingT80 -2.1.1 Embedded PipingA. Type: Single Layer Pex Barrier A, or Single Layer Pex Barrier B. Convert to Pex-Al-Pex at slab exit, and connect to Distribution pipe.B. Insulation: NoneC. Temperature Range: 0-90°CD. Joining Method: Compression FittingsE. Pipe Size: 20mm ODF. Fixing Concrete Slab: Pipes to be fixed on 10mm Rebar rod with cable ties. Rods to be raised with A-frame lattices of suitable height so that pipe network is on the neutral axis of the slab.G. Fixing Surface Bed: Pipes to be fixed on 10mm Rebar rod with cable ties. Rods to be fixed to mesh placed on top of isolation board.T80 -2.2 Embedded Line ComponentsT80 -2.2.1 Isolating Valves (<= 50mm)A. Type: Ball valve with nipples.B. Material: 1. Valve: PVC2. Nipples: PVC",null,0]
[]
["PART 3 - EXECUTION  T80 -1.1 Embedded Line  T80 -1.1.1 Preparation A. Lay bottom rebar. Do NOT proceed with top rebar until pipe coils are fixed. B. Ensure that the pressure pump system is operational and prepared to put all the coils under pressure for the duration of the casting process  T80 -1.1.2 Installation A. Fix A-frame lattices to bottom rebar with cable ties, every 400mm. Space lattices 1m apart, perpendicular to the coil direction and ensure it spans the entire width of the coil with an overhang of 200mm minimum at each side. B. Fix 10mm rebar rods perpendicular to the A-frame lattices, at the indicated pitch of the coils. Rods shall span the entire length of the coil. C. Fix the pipe to the rebar rod with cable ties every 400mm. Ensure that all cut ends are removed from the deck. D. A minimum bending radius of 250mm is required at each turn. E. Ensure that no-go areas around columns and slab edges are adhered to as per drawings. Pipes can simply be routed around these areas and pitched narrower for sections. F. Where pipes cross over construction joints, a 300mm long HDPE sleeve shall be put over the crossings. G. Where pipes need to penetrate through shutter boards, a 32mm hole shall be drilled, and a 250mm long 32mm HDPE sleeve slipped over the pipe end. The sleeve shall be plugged on the concrete side to ensure that concrete does not leak through during the pour. H. Where pipe end exit to ground manifolds, care shall be taken that pipes are not closer than 100mm from each other, in order not to create a honeycomb. I. Inspect the coils to ensure that the pipe is not pinched anywhere. J. Fix the top rebar only after the pipe coil are inspected and cleared of defects. K. Make up a temporary manifold an ensure all pipe coils are connected. L. Start the pressure pump system and bleed the air out of the system. M. Keep the system under pressure for the duration of the casting process, as well as during construction.  T80 -1.1.3 Temporary Pressure Pump System A. A temporary pressure pump system that can be easily moved on site, shall be used to put the pipe system under pressure from casting, and for the duration of the project. B. This is to ensure that should any damage occur on the embedded pipes, the leak can be found instantly and repaired before finishing is done. C. The system shall consist of a pressure pump that can deliver 0.5 L/s at 6 Bar pressure. D. A plastic buffer tank shall be used that will be connected to the suction side of the pump. E. The pump shall feed into the coils or distribution piping via temporary manifolds that will be made from 20mm Pex piping. Plasson type Tees can be used for connecting the temporary manifold. F. The return pipe shall feed back into the buffer tank and choked with a ball valve to ensure that air is bled form the system.  T80 -1.1.4 Protection A. Protect installed products until completion of project. B. Ensure that all open pipe ends are plugged in working areas, until connections are made. C. All drilling in slabs must be done with stopper sleeves over the drill bits to ensure that drill bits cannot penetrate deeper than 75mm into any surface with embedded pipes.  T80 -1.1.5 Delivery, Storage and Handling A. Store and handle in strict compliance with manufacturer's written instructions and recommendations. B. Protect from damage due to weather, excessive temperature, and construction operations.",null,0]
[]
["Applicable Drawings","H3",0]
[]
["135-MM001-T-00 BLOCK A LOWER GROUND FLOOR TABS DRW 1 OF 2",null,0]
[]
["135-MM002-T-00 BLOCK A LOWER GROUND FLOOR TABS DRW 2 OF 2",null,0]
[]
["135-MM003-T-00 BLOCK A GROUND FLOOR TABS DRW 1 OF 3",null,0]
[]
["135-MM004-T-00 BLOCK A GROUND FLOOR TABS DRW 2 OF 3",null,0]
[]
["135-MM005-T-00 BLOCK A GROUND FLOOR TABS DRW 3 OF 3",null,0]
[]
["135-MM006-T-00 BLOCK A FIRST FLOOR TABS DRW 1 OF 3",null,0]
[]
["135-MM007-T-00 BLOCK A FIRST FLOOR TABS DRW 2 OF 3",null,0]
[]
["135-MM008-T-00 BLOCK A FIRST FLOOR TABS DRW 3 OF 3",null,0]
[]
["135-MM009-T-00 BLOCK A SECOND FLOOR TABS DRW 1 OF 3",null,0]
[]
["135-MM010-T-00 BLOCK A SECOND FLOOR TABS DRW 2 OF 3",null,0]
[]
["135-MM011-T-00 BLOCK A SECOND FLOOR TABS DRW 3 OF 3",null,0]
[]
["135-MM012-T-00 BLOCK B LOWER GROUND FLOOR TABS DRW 1 OF 1",null,0]
[]
["135-MM013-T-00 BLOCK B GROUND FLOOR TABS DRW 1 OF 2",null,0]
[]
["135-MM014-T-00 BLOCK B GROUND FLOOR TABS DRW 2 OF 2",null,0]
[]
["135-MM015-T-00 BLOCK B FIRST FLOOR TABS DRW 2 OF 2",null,0]
[]
["135-MM016-T-00 BLOCK B FIRST FLOOR TABS DRW 1 OF 2",null,0]
[]
["135-MM017-T-00 BLOCK B SECOND FLOOR TABS DRW 1 OF 1",null,0]
[]
["135-MM018-T-00 BLOCK C GROUND FLOOR TABS  DRW 1 OF 2",null,0]
[]
["135-MM019-T-00 BLOCK C GROUND FLOOR TABS  DRW 2 OF 2",null,0]
[]
["135-MM020-T-00 BLOCK C FIRST FLOOR TABS DRW 1 OF 2",null,0]
[]
["135-MM021-T-00 BLOCK C FIRST FLOOR TABS DRW 2 OF 2",null,0]
[]
["135-MM022-T-00 BLOCK C SECOND FLOOR TABS DRW 1 OF 1",null,0]
[]
["135-MM023-T-00 BLOCK D GROUND FLOOR TABS DRW 1 OF 3",null,0]
[]
["135-MM024-T-00 BLOCK D GROUND FLOOR TABS DRW 2 OF 3",null,0]
[]
["135-MM025-T-00 BLOCK D GROUND FLOOR TABS DRW 3 OF 3",null,0]
[]
["135-MM026-T-00 BLOCK D FIRST FLOOR TABS DRW 1 OF 2",null,0]
[]
["135-MM027-T-00 BLOCK D FIRST FLOOR TABS DRW 2 OF 2",null,0]
[]
["135-MM028-T-00 BLOCK D SECOND FLOOR TABS DRW 1 OF 2",null,0]
[]
["135-MM029-T-00 BLOCK D SECOND FLOOR TABS DRW 2 OF 2",null,0]
[]
["135-MM030-T-00 BLOCK E KITCHEN AND LAUNDRY TABS DRW 1 OF 1",null,0]
[]
["PRELIMINARY AND GENERAL","H2",0]
[]
["Technical Submittals","Item",1,null,{"$f":"D10312*C10312","v":{"v":0,"d":"R0.00"}}]
[{"$nulls":4},{"$f":"D10313*C10313","v":{"v":0,"d":"R0.00"}}]
["Workshop drawings – Paper and electronic","Sets",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["As-Built Drawings – Paper and electronic","Sets",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Operating and Maintenance Manuals - Paper and electronic","Sets",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Warranty and maintenance per month","Months",12,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Training of Client's maintenance team","Days",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["T80 TABS: RATE TO INCLUDE SUPPLY, INSTALLATION, TESTING  & COMMISSIONING AS PER T80 PART 3","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Piping","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Embedded Piping","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Straight Pipe","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["20mm Pex","m",220000,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["20mm Pex-Al-Pex","m",4700,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Elbows","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["20mm Crimp","No",4500,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Embedded Line Components  – All line components to include fittings to connect to pipe.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Isolating Valves <=50mm","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["20mm Ball Valve with crimp fittings to Pex-Al-Pex.","No",3800,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TABS Installation","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Drilling of hole through shutterboard, with 200mm 32mm HDPE Sleeve.","No",2900,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Inspection of coils before Casting","No",1850,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Manifold Test. Labour portion only. Will consist of connecting coils in batches and to test with pressure unit. Include tests done during first fix, as well as second fix. Allowance made to test all slabs in 3 sections, 3 times in a row.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["A-Frame Stool: 80x130mm. 8mm Top and bottom bars. 5.6mm Side Support","m",60000,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["10mm Rebar Rod for fixing PEX piping","m",200000,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["7.8mm Cable Ties to fix pipe on mesh – one every 400mm","No",500000,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["7.8mm Cable Ties to strap mesh to bottom rebar","No",500000,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Temporary Pressure Pump System","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Pressure pump with 1000 liters tank needed to pressurise pipe systems","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["20mm Plasson T-s sacrificial fittings to connect to pipe manifold for testing. (Fitting can be used 3 times.)","No",1250,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Repairing first fix leak. Involve no breaking of concrete.","No",100,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Repairing second fix leak – will typically involve breaking of concrete.","No",250,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["LIST OF IMPORTED ITEMS: APPLICABLE ITEMS TO BE LISTED WITH MATERIALS PRICE OF ITEM, AS WELL AS THE EXCHANGE RATE THE PRICE IS BASED ON AT TIME OF TENDER","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SUBMITTALS REQUIRED AT TIME OF TENDER: THIS SHALL FIX THE EQUIPMENT OFFERED. ANY CHANGES TO THIS EQUIPMENT TO BE ONLY BY APPROVAL OF THE ENGINEER","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Technical Brochure: Pex Piping","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D10377*C10377","v":{"v":0,"d":"R0.00"}}]
["TOTAL SECTION 3 CARRIED TO FINAL SUMMARY",null,0,null,{"$f":"SUM(E10217:E10377)","v":{"v":0,"d":"0.00"}}]
[null,null,0,null,{"v":0,"d":"R0.00"}]
["SECTION 4","H2",0,null,{"$f":"D10380*C10380","v":{"v":0,"d":"R0.00"}}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["EXTERNAL WORKS (PROVISIONAL) ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["BILL NO 1","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["DEMOLITIONS ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PREAMBLES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Preambles for Trades as defined in Scope of Work (C3.1 Item 4.1 & Item 4.2)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TRADE NAMES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Any reference to trade names in the Bills of Quantities or  Architect's specification or drawings shall deem to mean \"or similar and approved\"",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 104 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["DEMOLITIONS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["All material become the property of the Contractor and are to be removed by him from the site.  All debris and rubbish arising from the demolitions are to be immediately carted away and the site left clear and unencumbered","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Any breaking up, breaking down, etc. and removal of existing work must be done with the greatest care to prevent any form of structural or other damage to work or items not due to be removed. If any such damage may occur it will be made good by the Contractor on his own expense","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["REMOVAL OF TREES ETC","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Taking out and removing, grubbing up roots and filling in holes, for removal of trees","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cutting down and removing trees exceeding 200mm and not exceeding 500mm girth, including grubbing up roots, all necessary filling in of holes, lightly compacted and roughly levelled","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but exceeding 500mm and not exceeding 1000mm girth","No",8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but exceeding 1500mm and not exceeding 2000mm girth","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but exceeding 2000mm and not exceeding 2500mm girth","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but exceeding 2500mm and not exceeding 3000mm girth","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["EXTERNAL ROAD AND TRAFFIC CIRCLE","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Break down and remove existing single storey building with double pitch sloping roof approximately 15m2 on plan and average 3.00m high, comprising of 100mm thick concrete surface bed, one brick external walls, mainly half brick internal walls and corrugated iron steel roof covering on timber structure complete with foundations, windows, doors, etc., including any necessary excavations, filling, compaction, roughly levelling ground surface, carting away, etc ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Taking out and removing, grubbing up roots and filling in holes","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cutting down and removing trees exceeding 200mm and not exceeding 500mm girth, including grubbing up roots, all necessary filling in of holes, lightly compacted and roughly levelled","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but exceeding 500mm and not exceeding 1000mm girth","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but exceeding 1500mm and not exceeding 2000mm girth","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["BREAKING UP AND REMOVING","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Break up and remove existing 80mm thick concrete block paving on sand bedding ","m2",468,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Break up and remove existing tarmac, not exceeding 50mm thick including preparation, roughly levelling ground surfaces, ramming, etc. including saw cutting of existing premix to form clean neat joint on reinstatement","m2",10843,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Break up and remove existing precast concrete rainwater channel 150mm wide including preparation, roughly levelling ground surfaces, ramming, etc.","m",355,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Break up and remove existing in-situ cast concrete trapezoidal rainwater channel 3000mm wide and 100mm thick including preparation, roughly levelling ground surfaces, ramming, etc.","m",270,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clean existing stormwater channel","m",218,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Saw cut existing asphalt and tie into existing road surfacing","m",38,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D10443*C10443","v":{"v":0,"d":"R0.00"}}]
["Taking out and remove existing valve, meter, etc chambers size 225 x 225 x 600mm deep including compacted filling, etc","m",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Clean and flush out existing 110mm stormwater pipes to be cleared of all debris","m",200,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Break down and remove existing storm water catchpit, size approximately 1000 x 1000 x 1500mm deep under ground level, complete with overslab, floor channels, etc. including necessary excavations, filling, compaction, roughly levelling ground surface, etc.","m",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Break down and remove existing storm water kerb inlet, size approximately 2500 x 3000 x 1500mm deep under ground level, complete with overslab, etc.  including necessary excavations, filling, compaction, roughly levelling ground surface, etc.","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Break down and remove existing sewer manhole, size approximately 1000 x 1000 x 1000mm deep under ground level, complete with over slab, floor channels, etc.  including necessary excavations, filling, compaction, roughly levelling ground surface, etc.","m",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Break up and remove existing precast concrete kerb, over all size approximately 300 x 150mm wide, including necessary excavations, filling, compaction, roughly levelling ground surface, etc.","m",821,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Break up and remove existing precast concrete rainwater channel 150mm wide including preparation, roughly levelling ground surfaces, ramming, etc.","m",24,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Break down and remove existing stock fence, approximately 1500mm high, complete with all timber posts, single gate,  concrete footings, concrete underdig, etc. including necessary excavations, filling, compaction, roughly levelling, etc.","m",125,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Break down and remove existing road sign, approximately 2400mm high, complete with post,  concrete footing, etc. including necessary excavations, filling, compaction, roughly levelling, etc. ","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Remove existing steel gate, size 3000 x 2100mm high,  including any concrete footings, excavations, filling, compaction, roughly levelling, etc.necessary excavations, filling, compaction,  roughly levelling ground surface, carting away","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["EXTERNAL ROAD SUID STREET CROSSING - WIDENING OF ROAD","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["BREAKING UP AND REMOVING","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Break up and remove existing 60mm thick concrete block sidewalk paving on sand bedding ","m2",1095,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Break up and remove existing tarmac, not exceeding 50mm thick including preparation, roughly levelling ground surfaces, ramming, etc. including saw cutting of existing premix to form clean neat joint on reinstatement","m2",876,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Break down and remove existing storm water catchpit, size approximately 1000 x 1000 x 1500mm deep under ground level, complete with overslab, floor channels, etc.  including necessary excavations, filling, compaction, roughly levelling ground surface, etc.","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Break up and remove existing precast concrete kerb, over all size approximately 300 x 150mm wide, including necessary excavations, filling, compaction, roughly levelling ground surface, etc.","m",457,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TOTAL DEMOLITIONS ",null,0,null,{"$f":"SUM(E10379:E10475)","v":{"v":0,"d":"0.00"}}]
[null,null,0,null,{"v":0,"d":"R0.00"}]
["SECTION 4","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["EXTERNAL WORKS (PROVISIONAL)","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["BILL NO 2","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["GENERAL SITE WORKS, ROADS AND PAVING ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PREAMBLES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Preambles for Trades as defined in Scope of Work (C3.1 Item 4.1 & Item 4.2)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TRADE NAMES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Any reference to trade names in the Bills of Quantities or  Architect's specification or drawings shall deem to mean \"or similar and approved\"",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Nature of ground","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["A soils investigation has been carried out on site by the engineer and the report is available for inspection at the offices of the engineers. Descriptions of excavations shall be deemed to include all ground conditions classifiable as \"earth\" described in the above report and where conditions of a more difficult character are indicated these are separately measured",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Carting away of excavated material","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Descriptions of carting away of excavated material shall be deemed to include loading excavated material onto trucks directly from the excavations or, alternatively, from stock piles situated on the building site",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SUPPLEMENTARY PREAMBLES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE :All Civil works to be carried out in accordance with the standardised SABS 1200 specifications",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The Tenderer is referred to Section 4 and the JBCC CPAP workgroups for similar items, which will apply equally to the work in this Bill unless otherwise described.",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D10507*C10507","v":{"v":0,"d":"R0.00"}}]
["NOTE: The following items shall be deemed to fall into Work Group No 154 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SITE CLEARANCE ETC ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Site clearance","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Note:  The costs of soil, compaction, etc. tests in accordance with SABS 1200 are to be included in the rates for the relevant works","H4",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for 15 x 15m maximum grid survey after removal of topsoil (before platform construction commences)","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for 15 x 15m maximum grid survey of completed platform (after platform construction)","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Digging up and removing rubbish, debris, vegetation, hedges, shrubs and trees not exceeding 200mm girth, bush, etc","m2",163301,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Stripping average 200mm thick layer of top soil and stockpiling on site not exceeding 500m from the perimeter of excavations","m3",24496,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Selected top soil obtained from the stockpiles on site, including haulage not exceeding 500m from the perimeter of  stock pile in layers of 100mm, spread levelled over site","m3",24496,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["BULK EXCAVATION, ETC ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Open face excavation in earth over sloping site ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavate in all material to form platforms and stockpile on site including not exceeding 500m from the excavations ","m3",63591,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but to form attenuation pond","m3",7072,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but to form courtyards","m3",223,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but for service tunnel excavation ","m3",13905,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over bulk excavation in earth for excavation in","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Intermediate rock in platforms, roads and parking areas (stockpile separate from normal excavations for crushing later)","m3",14744,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Hard rock in various platforms, roads and parking areas (stockpile separate from normal excavations for crushing later) ","m3",27714,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["CRUSHING","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Crushing of selected rock material obtained from the stock piles and crushed by means of multi-stage crushing, for the crushed material to comply to the minimum G7 specification ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Crushed material","m3",25409,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Crushing of selected rock material obtained from the stock piles and crushed by means of multi-stage crushing, for the crushed material to comply to the minimum G5 specification ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Crushed material","m3",17049,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["FILLING  ETC.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blend/mix material excavated during bulk excavations (free of organic matter) with minimum proportion of 35% “soft excavated material” and 65% “crushed rock material” obtained from stockpile, compacted to a minimum of 95% Mod AASHTO density. (minimum of four compaction tests per maximum of 500m³).","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fill to platform","m3",39348,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but to attenuation pond berms","m3",215,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but to bottom of service tunnel ","m3",10,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Selected crushed material  from the stock piles,  to comply with the minimum specification of G7 and compacted in layers not exceeding 150mm to 95%  modified AASHTO ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fill to platform ","m3",2760,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["CARTING AWAY, COMPACTION, ETC.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavated filling obtained from the stockpiles on site, including haulage not exceeding 500m from the perimeter of  stock pile, in layers of 100mm, spread levelled over site","m3",21667,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D10571*C10571","v":{"v":0,"d":"R0.00"}}]
["Extra over all excavations for carting away","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Surplus material from excavations and/or stock piles on site to a dumping site to be located by the contractor","m3",2815,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Compaction of surfaces ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Compaction of ground including scarifying for a depth of 150mm, breaking down oversize material, adding suitable material where necessary and compacting to 90% Mod AASHTO density","m2",116569,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Keeping excavations free of water","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Keeping excavations free of water in all excavations in External Works","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["STONE LAYER UNDER LOWER GROUND PARKING AREA","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Approved 19mm Stone layer under lower ground parking area imported from commercial sources supplied and carted on by the Contractor","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["250mm Thick 19mm stone layer under basement parking area","m3",1679,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["THE FOLLOWING IN INTERNAL ROADS AND PARKING AREAS ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TREATMENT OF ROADBED","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Roadbed preparation, scarify earth surface to a depth of 150mm, breaking down over size material and reconsolidate to 93% modified AASHTO density ","m2",47661,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Selected crushed material  from the stock piles, for the purpose of fill, to comply to the minimum specification of G7 compacted in layers not exceeding 150mm to 93%  modified AASHTO density ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Road layer works ","m3",4433,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Selected crushed material  from the crushed stock piles, for the purpose of fill, to comply to the minimum specification of G5, for the purpose of subbase, including stabilizing agent to reach C3, compacted in layers not exceeding 150mm to 97% Mod. AASHTO density","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150mm Thick sub base ","m3",4433,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Approved G2 basecourse material imported from commercial sources supplied and carted on by the Contractor, compacted in layers not exceeding 150mm to 98% density","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150mm Thick base","m3",3537,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Selected crushed material  from the crushed stock piles, for the purpose of fill to comply to the minimum specification of G5, for the purpose of subbase fill including stabilizing agent to reach C4, compacted in layers not exceeding 150mm to 97% Mod. AASHTO density","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["120mm Thick sub base ","m3",2097,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Selected crushed material  from the crushed stock piles, for the purpose of fill to comply to the minimum specification of G5, for the purpose of subbase fill stabilized agent to reach C3 supplied and carted on by the Contractor, compacted in layers not exceeding 150mm to 97% Mod. AASHTO density","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["120mm Thick sub base ","m3",2097,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Approved G5 filling supplied and carted on by the Contractor, compacted in layers not exceeding 150mm to 97% Mod. AASHTO density","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100mm Thick sub base under sidewalk paving","m3",63,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["20mm River sand ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Under paving ","m2",5334,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SEGMENTED PAVING INTERLOCKING PRECAST CONCRETE PAVING","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Grey interlocking precast concrete paving blocks type SA, including all cutting of units to fit between edge restraints, laid on and including 20mm riversand bed, compacted and plaster sand broomed into joints on completion","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["60mm To sidewalks","m2",630,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["80mm To roads","m2",22809,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["ASPHALT BASE AND SURFACING","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Prime coat using","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D10635*C10635","v":{"v":0,"d":"R0.00"}}]
["MC-30 cut-back bitumen","m2",23578,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Tack coat using","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["30% Cationic stable grade emulsion","m2",23578,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Continuously graded TPA medium asphalt with 50/70 penetrating grade bitumen binder","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["40mm Thick","m2",23578,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Saw-cutting of asphalt base or paving","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["40mm Thick asphalt surfacing","m",1867,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["KERBING, CHANNELLING, EDGE BEAMS, ETC","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PRECAST CONCRETE KERBING","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fig 4 kerbing","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150 x 250mm Barrier kerb as SABS Specification 927 Fig.4, in approximately 1000mm lengths, bedded, jointed and pointed including unreinforced concrete foundation size 300 x 75mm thick under and 200 x 200 x 180mm high unreinforced concrete Class B haunching behind, including necessary excavation","m",6355,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but circular on plan not exceeding 4,0m radius","m",229,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but circular on plan exceeding 4,0m radius","m",1816,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150 x 250mm Dropped barrier kerb as SABS Specification 927 Fig.4, in approximately 1000mm lengths, bedded, jointed and pointed including unreinforced concrete foundation size 300 x 75mm thick under, dropped 230mm below road level haunching behind, including necessary excavation","m",91,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fig 14 channelling","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["125 x 300mm Precast concrete channel as SABS Specification 927 Fig.14, in approximately 1000mm lengths, bedded, jointed and pointed in 1:3 cement mortar, including unreinforced concrete foundation size 450 x 75mm thick under and 200 x 200 x 180mm high unreinforced concrete Class B haunching behind, including necessary excavation","m",3001,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but circular on plan not exceeding 4,0m radius","m",15,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but circular on plan exceeding 4,0m radius","m",448,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Concrete edge beam","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150 x 100mm Concrete edge beam of class 20/19mm concrete ","m",88,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TRAFFIC SIGNS MEASURED IN NUMBER ANCILLARY ROADWORKS TRAFFIC SIGNS ERECTED COMPLETE","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Statutory signs, street names, etc supplied and erected complete, including posts, excavation, etc","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Provision and erection of regulatory traffic signs for 60km/h design standard, complete","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Stop sign (R1)","No",20,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["4-Way Stop sign (R1.4)","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Proceed left only road sign (R105)","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Yield sign (R2)","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Yield at traffic circle sign (R2.2)","No",7,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Speed limit (R201-40)","No",9,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Keep left road (R103)","No",11,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Motor cycle parking reservation road sign (R307-P)","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Bicycle parking reservation road sign (R304-P)","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D10699*C10699","v":{"v":0,"d":"R0.00"}}]
["Parking reservation road sign (R305-P)","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Disabled persons parking reservation road sign (R305-P)","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Road sign (GDS21)","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["No unauthorized vehicles (R208)","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["No entry sign (R3)","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Road sign (IN4)","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Two way traffic road sign (W212)","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Location of fire fighting equipment road sign (FB1)","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sharp curve right road sign (W204)","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["No parking / Loading bay sign","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["No parking sign (R216)","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Busses/taxi sign (R134)","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Provision and erection of warning traffic signs for 60km/h design standard, complete","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Traffic circle (W201)","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Single sharp curve chevron (W405/6)","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Triple sharp curve chevron (W408)","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Gore chevron sign (W413)","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["ROAD MARKINGS","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["RETRO-REFLECTIVE ROAD MARKINGS","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Prepare and paint two coats approved roadmarking paint:","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["White lines ( broken or unbroken )","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100mm Wide broken lines GM1 reduced lane lines","m",124,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100mm Wide broken lines GM1 Standard lane lines","m",545,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100mm Wide broken lines GM1 Extra lane lines","m",98,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150mm Wide solid dividing line WM3","m",230,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["200mm Wide RTM2 Yield line with 600 - 300mm line gap ","m",169,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["300mm Wide RTM1 stop line","m",100,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100mm Wide RM3 Channelizing line","m",16,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100mm Wide continuous roadmarking line for parking bays","m",2502,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Disabled persons symbol","No",8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Single headed directional arrow 400mm wide x 1400mm long","No",12,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Yellow lines ( broken or unbroken )","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D10763*C10763","v":{"v":0,"d":"R0.00"}}]
["100mm Lines RM5  for painted islands","m",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100mm Lines for loading zone bays","m",179,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150mm Lines","m",88,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["White characters","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Straight arrows WM7.3 4000mm long","No",48,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Right arrows WM7.5 4000mm long","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Left arrows WM7.1 4000mm long","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Bifunction arrows (straight and right) WM7.2 4000mm long","No",9,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Bifunction arrows (straight and left) RM7.2  4000mm long","No",7,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Trifunction arrows 4000mm long","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["White characters and symbols","m2",25,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Yellow characters and symbols","m2",22,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Traffic island markings (any colour)","m2",22,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["White characters (Stop sign lettering painted on road RTW1 )","No",10,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Yield control ahead arrow WM5 2500mm long","No",13,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Yellow characters (Loading zone icon painted on road)","No",7,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["ACCOMMODATION OF TRAFFIC","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Accommodation of traffic during construction (4 months) ","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["EXTERNAL ROAD SUID STREET CROSSING - WIDENING OF ROAD","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["MILLING","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Milling out existing bituminous material with an average depth of:  This rate shall include milling, loading, transporting and disposing of material at an approve dump site located by the contractor. Rate for site establishment and de-establishment to be included in the rate provided.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Exceeding 30mm but not exceeding 60mm","m2",876,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["EARTHWORKS","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Open face excavation in compacted layer works ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavate to reduce levels under road and spoil at dump site located by contractor ","m3",429,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavate to reduce levels under sidewalk paving and and spoil at dump site located by contractor ","m3",110,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TREATMENT OF ROADBED","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Roadbed preparation, scarify earth surface to a depth of 150mm, breaking down over size material and reconsolidate to 93% modified AASHTO density ","m2",2196,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Selected crushed material  from the crushed stock piles, for the purpose of fill, to comply to the minimum specification of G7 compacted in layers not exceeding 150mm to 97%  modified AASHTO density ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Road layer works ","m3",165,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Selected crushed material  from the crushed stock piles, for the purpose of fill, to comply to the minimum specification of G5, for the purpose of subbase, including stabilizing agent to reach C3, compacted in layers not exceeding 150mm to 97% Mod. AASHTO density","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150mm Thick sub base ","m3",165,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D10827*C10827","v":{"v":0,"d":"R0.00"}}]
["Approved G2 basecourse material imported from commercial sources supplied and carted on by the Contractor, compacted in layers not exceeding 150mm to 98% density","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150mm Thick base","m3",131,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Approved G5 filling supplied and carted on by the Contractor, compacted in layers not exceeding 150mm to 97% Mod. AASHTO density","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100mm Thick sub base under sidewalk paving","m3",110,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SEGMENTED PAVING INTERLOCKING PRECAST CONCRETE PAVING","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Grey interlocking precast concrete paving blocks type SA, including all cutting of units to fit between edge restraints, laid on and including 20mm riversand bed, compacted and plaster sand broomed into joints on completion","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["60mm To sidewalks","m2",1095,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["ASPHALT BASE AND SURFACING","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Prime coat using","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["MC-30 cut-back bitumen","m2",876,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Tack coat using","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["30% Cationic stable grade emulsion","m2",876,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Continuously graded TPA medium asphalt with 50/70 penetrating grade bitumen binder","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["40mm Thick","m2",876,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SAW CUTTING","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Saw-cutting of asphalt base or paving","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["40mm Thick asphalt surfacing","m",80,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["KERBING, CHANNELLING, EDGE BEAMS, ETC","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PRECAST CONCRETE KERBING","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fig 4 kerbing","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150 x 250mm Barrier kerb as SABS Specification 927 Fig.4, in approximately 1000mm lengths, bedded, jointed and pointed including unreinforced concrete foundation size 300 x 75mm thick under and 200 x 200 x 180mm high unreinforced concrete Class B haunching behind, including necessary excavation","m",457,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but circular on plan not exceeding 4,0m radius","m",55,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but circular on plan exceeding 4,0m radius","m",72,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fig 14 channelling","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["125 x 300mm Precast concrete channel as SABS Specification 927 Fig.14, in approximately 1000mm lengths, bedded, jointed and pointed in 1:3 cement mortar, including unreinforced concrete foundation size 450 x 75mm thick under and 200 x 200 x 180mm high unreinforced concrete Class B haunching behind, including necessary excavation","m",457,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but circular on plan not exceeding 4,0m radius","m",55,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but circular on plan exceeding 4,0m radius","m",72,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Concrete edge beam","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150 x 100mm Concrete edge beam of class 20/19mm concrete ","m",457,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TRAFFIC SIGNS MEASURED IN NUMBER ANCILLARY ROADWORKS TRAFFIC SIGNS ERECTED COMPLETE","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Statutory signs, street names, etc supplied and erected complete, including posts, excavation, etc","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Provision and erection of regulatory traffic signs for 60km/h design standard, complete","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D10891*C10891","v":{"v":0,"d":"R0.00"}}]
["Speed limit (R201)","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Busses/minibusses (R136)","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["No parking sign (R216)","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Busses/taxi sign (R134)","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["RETRO-REFLECTIVE ROAD MARKINGS","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Prepare and paint two coats approved roadmarking paint:","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["White lines ( broken or unbroken )","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100mm Wide broken lines GM1 reduced lane lines","m",55,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100mm Wide broken lines GM1 Standard lane lines","m",1887,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100mm Wide broken lines GM1 Extra lane lines","m",92,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150mm Wide solid dividing line WM3","m",988,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["200mm Wide RTM2 Yield line with 600 - 300mm line gap ","m",25,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["300mm Wide RTM1 stop line","m",21,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100mm Wide RM3 Channelizing line","m",52,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["White characters","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Right arrows WM7.5 4000mm long","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Bifunction arrows (straight and right) WM7.2 4000mm long","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Bifunction arrows (straight and left) RM7.2  4000mm long","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Bifunction arrows GM3.3 4000mm long","No",12,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["ACCOMMODATION OF TRAFFIC","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Accommodation of traffic during construction ","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["MAIN ENTRANCE EXTERNAL ROAD AND TRAFFIC CIRCLE","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SITE CLEARANCE ETC ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Digging up and removing rubbish, debris, vegetation, hedges, shrubs and trees not exceeding 200mm girth, bush, etc","m2",14091,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Stripping average 200mm thick layer of top soil and stockpiling on site","m3",3233,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Selected top soil obtained from the stockpiles on site, including haulage not exceeding 1000m for the perimeter of  stock pile in layers of 100mm, spread levelled over site","m3",3233,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["BULK EXCAVATION, ETC ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Note:  The costs of soil, compaction, etc. tests in accordance with SABS 1200 are to be included in the rates for the relevant works","H4",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Open face excavation in earth for boxcutting in road","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavation in \"earth\" under parking areas, buildings, etc. to reduce levels and depositing excavated material in prescribed stock piles on site not exceeding 500m from the excavations ","m3",3676,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavation in \"earth\" not exceeding 2m deep to remove unsuitable material and load and cart away from site","m3",3233,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Compaction of surfaces ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D10955*C10955","v":{"v":0,"d":"R0.00"}}]
["Compaction of ground including scarifying for a depth of 150mm, breaking down oversize material, adding suitable material where necessary and compacting to 90% Mod AASHTO density","m2",14091,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["FILLING  ETC.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Earth filling obtained from the prescribed stock piles on site including haulage not exceeding 500m from perimeter of excavations or stock piles compacted in layers not exceeding 150mm to 95%  modified AASHTO density ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fill for road and traffic circle","m3",3676,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["THE FOLLOWING IN EXTERNAL ROADS AND TRAFFIC CIRCLE","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TREATMENT OF ROADBED","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Roadbed preparation and compaction of material to minimum 93% mod AASHTO density","m2",14091,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Selected crushed material  from the crushed stock piles, for the purpose of subbase fill, to comply to the minimum specification of G7 compacted in layers not exceeding 150mm to 93%  modified AASHTO density ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150mm Thick sub-base ","m3",1699,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Selected crushed material  from the crushed stock piles, for the purpose of fill, to comply to the minimum specification of G5, for the purpose of subbase fill, including stabilizing agent to reach C3, compacted in layers not exceeding 150mm to 97% Mod. AASHTO density","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150mm Thick sub base ","m3",1699,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Approved G2 basecourse material from excavated  crushed stone material supplied and carted on by the Contractor, compacted in layers not exceeding 150mm to 98% density","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150mm Thick base","m3",1483,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Selected crushed material  from the crushed stock piles, for the purpose of fill, to comply to the minimum specification of G5, for the purpose of subbase fill, including stabilizing agent to reach C4, compacted in layers not exceeding 150mm to 97% Mod. AASHTO density","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["120mm Thick sub base ","m3",304,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Selected crushed material  from the crushed stock piles, for the purpose of fill to comply to the minimum specification of G5, for the purpose of subbase fill including stabilizing agent to reach C3 supplied and carted on by the Contractor, compacted in layers not exceeding 150mm to 97% Mod. AASHTO density","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["120mm Thick sub base ","m3",304,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SEGMENTED PAVING INTERLOCKING PRECAST CONCRETE PAVING","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Grey interlocking precast concrete paving blocks type SA, including all cutting of units to fit between edge restraints, laid on and including 20mm riversand bed, compacted and plaster sand broomed into joints on completion","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["60mm To sidewalks","m2",2534,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["ASPHALT BASE AND SURFACING","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Prime coat using","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["MC-30 cut-back bitumen","m2",9886,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Tack coat using","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["30% Cationic stable grade emulsion","m2",9886,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Continuously graded TPA medium asphalt with 50/70 penetrating grade bitumen binder","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["40mm Thick","m2",9886,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Saw-cutting of asphalt base or paving","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["40mm Thick asphalt surfacing","m",554,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["KERBING, CHANNELLING, EDGE BEAMS, ETC","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PRECAST CONCRETE KERBING","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fig 4 kerbing","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D11019*C11019","v":{"v":0,"d":"R0.00"}}]
["150 x 250mm Barrier kerb as SABS Specification 927 Fig.4, in approximately 1000mm lengths, bedded, jointed and pointed including unreinforced concrete foundation size 300 x 75mm thick under and 200 x 200 x 180mm high unreinforced concrete Class B haunching behind, including necessary excavation","m",692,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but circular on plan not exceeding 4,0m radius","m",26,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but circular on plan exceeding 4,0m radius","m",980,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fig 10 kerbing","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100 x 250mm High Figure 10 precast concrete kerb in approximately 1000mm lengths, bedded, jointed and pointed including unreinforced concrete foundation size 350 x 150mm thick under, and 200 x 200 x 200mm high unreinforced concrete Class B haunching behind including necessary excavation","m",249,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fig 14 channelling","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["125 x 300mm Precast concrete channel as SABS Specification 927 Fig.14, in approximately 1000mm lengths, bedded, jointed and pointed in 1:3 cement mortar, including unreinforced concrete foundation size 450 x 75mm thick under and 200 x 200 x 180mm high unreinforced concrete Class B haunching behind, including necessary excavation","m",565,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but circular on plan exceeding 4,0m radius","m",372,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Concrete edge beam","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150 x 100mm Concrete edge beam of class 20/19mm concrete ","m",110,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TRAPEZOIDAL CHANNEL","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavation in earth or compacted filling not exceeding 2m deep","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Reducing levels to final levels under new trapezoidal channel","m3",265,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Open trapezoidal shaped stormwater channels, laid to even falls, in sections not exceeding 3m, finished smooth to all visible faces, slightly rounded on salient angles","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Open trapezoidal shaped storm water channel, bottom 600mm wide x top 3000mm wide, to form 400mm deep channel consisting of 100mm thick in-situ cast Class 20/19 concrete ","m",249,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Approved G5 filling supplied and carted on by the Contractor, compacted in layers not exceeding 150mm to 95% Mod. AASHTO density","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Under stormwater channels","m3",224,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Compaction of surfaces ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Compaction of ground surface under surface beds etc including scarifying for a depth of 150mm, breaking down oversize material, adding suitable material where necessary and compacting to 93% Mod AASHTO density","m2",747,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fabric reinforcement","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Type 395 fabric reinforcement in concrete surface bed, slabs, etc.","m2",1047,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Expansion joint formed of bitumen impregnated soft board or jointex  ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["12mm Thick polystyrene joint filler between horizontal concrete surfaces not exceeding 300 mm high or wide","m",75,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TRAFFIC SIGNS MEASURED IN NUMBER ANCILLARY ROADWORKS TRAFFIC SIGNS ERECTED COMPLETE","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Statutory signs, street names, etc supplied and erected complete, including posts, excavation, etc","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Provision and erection of regulatory traffic signs for 60km/h design standard, complete","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Yield sign (R2)","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Proceed left only road sign (R105)","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Yield at traffic circle sign (R2.2)","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Speed limit (R201)","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Busses/minibusses (R136)","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Provision and erection of warning traffic signs for 60km/h design standard, complete","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D11083*C11083","v":{"v":0,"d":"R0.00"}}]
["Traffic circle (W201)","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Single sharp curve chevron (W405/6)","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Triple sharp curve chevron (W408)","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Gore chevron sign (W413)","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["RETRO-REFLECTIVE ROAD MARKINGS","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Retro-reflective paint applied at a nominal rate of 0,42l/m²","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["White lines ( broken or unbroken )","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100mm Wide broken lines GM1 reduced lane lines","m",729,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100mm Wide broken lines GM1 Standard lane lines","m",237,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100mm Wide broken lines GM1 Extra lane lines","m",68,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150mm Wide solid dividing line WM3","m",522,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["200mm Wide RTM2 Yield line with 600 - 300mm line gap ","m",119,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100mm Wide RM3 Channelizing line","m",80,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Yellow lines ( broken or unbroken )","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100mm Lines RM5  for painted islands","m",72,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["White characters","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Yield control ahead arrow WM5 2500mm long","No",8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Bifunction arrows GM3.3 4000mm long","No",24,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["White characters and symbols","m2",12,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Yellow characters and symbols","m2",10,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Traffic island markings (any colour)","m2",8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["ACCOMMODATION OF TRAFFIC","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Accommodation of traffic during construction ","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["THE FOLLOWING IN BLOCK RETAINING WALL - SOUTHERN BOUNDARY ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavation in earth or compacted filling not exceeding 2m deep","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Trenches","m3",169,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over all excavations for carting away","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Surplus material from excavations and/or stock piles on site to a dumping site to be located by the contractor","m3",17,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Back excavation of vertical sides of excavation in earth, for working space, including backfilling compacted to 93% Mod AASHTO density ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Not exceeding 1.5m deep approximately 1,5m away from face of building including backfilling and compaction to 93% mod AASHTO density ","m3",87,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Risk of collapse of excavations","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sides of trench and hole excavations exceeding 1,5m deep","m2",56,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D11147*C11147","v":{"v":0,"d":"R0.00"}}]
["Selected earth filling obtained from the excavations and/or prescribed stock piles on site in layers of 150mm thick compacted to 93% Mod AASHTO density","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Backfilling to trenches, holes, etc","m3",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Well drained sand supplied and carted on by the contractor, compacted to 100% Mod AASHTO density","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Backfilling behind retaining wall","m3",93,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["15MPa/19mm Unreinforced concrete","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blinding under retaining wall footings on excavated surfaces","m3",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["25 MPa/19 mm Reinforced concrete in","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Retaining wall footings","m3",17,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Mild steel reinforcement ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["8 mm Diameter bars","t",0.2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["High tensile steel rod reinforcement to structural concrete work","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["10mm Diameter bars","t",0.41,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["12mm Diameter bars","t",0.61,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["16mm Diameter bars","t",0.82,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Subsoil drain","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Subsoil drain formed with 75mm UPVC perforated geopipe, 550mm long, and through wall, inside 300 x 300 x 19mm stone drain consisting of 19mm nominal size crushed stone  including wrapping stone drain in A4 geotextile material","No",50,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["MVA7 BLOCK WALL (Supplier contact number:012-386 0058)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["MVA7 or equal approved blocks size 470 x 180 x 300mm high, and 38kg per block installed strictly according to manufacturer's specifications to be used in conjunction with slider panel blocks (slider panels blocks elsewhere measured)","No",1075,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Slider panels or equal approved size 395 x 175 x 40mm high, and 6.5kg per block installed strictly according to manufacturer's specifications to be used in conjunction with MVA7 blocks (MVA7 blocks elsewhere measured)","No",944,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["THE FOLLOWING IN CONCRETE RETAINING WALLS - NORTHERN BOUNDARY - TO BE CONSTRUCTED BEFORE PLATFORM IS CREATED","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavation in earth or compacted filling not exceeding 2m deep","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Trenches","m3",353,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over all excavations for carting away","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Surplus material from excavations and/or stock piles on site to a dumping site to be located by the contractor","m3",353,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Risk of collapse of excavations","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sides of trench and hole excavations exceeding 1,5m deep","m2",504,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Selected earth filling obtained from the excavations and/or prescribed stock piles on site in layers of 150mm thick compacted to 93% Mod AASHTO density","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Backfilling to trenches, holes, etc","m3",101,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Well drained sand supplied and carted on by the contractor, compacted to 93% Mod AASHTO density","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Backfilling behind retaining wall","m3",170,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["15MPa/19mm concrete","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blinding under strip footings on excavated surfaces","m3",29,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D11211*C11211","v":{"v":0,"d":"R0.00"}}]
["25 MPa/19 mm concrete in","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Retaining wall footings, stepped and level","m3",176,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Retaining walls, stepped and level","m3",236,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Rough formwork to sides","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Retaining walls","m2",1886,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Retaining wall footings","m2",252,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Mild steel reinforcement ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["8 mm Diameter bars","t",4.94,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["High tensile steel rod reinforcement to structural concrete work","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["10mm Diameter bars","t",14.83,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["12mm Diameter bars","t",12.36,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["16mm Diameter bars","t",17.3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Subsoil drain","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["A2 bidum geotextile material","m2",1130,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Kaytech or other equal approved \"Flow-drain\" fixed to back of retaining walls ","m2",565,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Subsoil drain formed with 110mm UPVC perforated geopipe, wrapped in A2 bidum geotextile material","m",420,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Expansion joints formed of jointex","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["10mm Jointex in vertical joint between concrete surfaces not exceeding 300mm high or wide","m",103,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Grey polysulphide sealant, including bond breaker, primer, etc ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["10mm Wide x 10mm deep in expansion joints ","m",206,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Apply 12mm thick cement plaster 1:4 mixture to concrete in one operation with steel trowel. Smooth and prepare surfaces and remove all loose material, and rinse","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On retaining walls","m2",1195,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Narrow widths","m2",105,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Prepare surfaces and remove all loose material and rinse.  Surfaces to be dry, sound and clean and cured for stipulated 28 or 14 days as stated with a moisture content, measured with a Doser Hygrometer of BD 2 scale - 8%.  Apply with one coat unreduced 100% pure acrylic emulsion water based Versus primer with two coats 100% pure acrylic water based Versus Aqua Ripple paint enhanced with marble aggregate, fillers and fungicides or similar approved.  All to manufacturer’s detailed specifications. TVOC limits (g/L of product) to be compliant to TVOC limits in Table IEQ13.1 for Green Star PEB - Custom Healthcare. Colour to Architect’s selection (Ref. C5)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["External walls","m2",1300,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PLAZA","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["EARTHWORKS","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavation in earth or compacted filling not exceeding 2m deep","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Trenches","m3",383,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Reduced levels under paving etc","m3",2452,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over all excavations for carting away","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over all excavations for carting surplus excavated material ","m3",2629,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D11275*C11275","v":{"v":0,"d":"R0.00"}}]
["Risk of collapse of excavations","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sides of trench and hole excavations not exceeding 1,5m deep","m2",947,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Selected earth filling obtained from the excavations and/or prescribed stock piles on site in layers of 150mm thick compacted to 93% Mod AASHTO density","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Backfilling to trenches, holes, etc","m3",206,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Compaction of surfaces ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Scarify earth surface to a depth of 150mm, breaking down over size material and reconsolidate to 90% modified AASHTO density ","m2",1496,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["G5 gravel layers supplied by the contractor compacted to 97% Mod AASHTO density in layers not exceeding 150mm ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Subbase under paving","m3",224,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["30 MPa/19 mm Reinforced concrete in","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Retaining walls","m3",65,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Strip footings","m3",52,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Seating slab","m3",15,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Stairs including landings, beams and inverted beams","m3",12,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sundries","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["20mm round edge to concrete","m",245,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Mild steel rod reinforcement to structural concrete ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["8mm Diameter bars","t",3.23,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["High tensile steel rod reinforcement to structural concrete ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["10mm Diameter bars","t",3.23,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["12mm Diameter bars","t",3.23,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["16mm Diameter bars","t",3.23,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["20mm Diameter bars","t",3.23,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fabric reinforcement","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Type 245 fabric reinforcement in concrete surface beds, slabs, etc.","m2",151,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Finishing top surface of concrete smooth with a wood float ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Surface beds, slabs, etc","m2",151,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Rough formwork to sides","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sloping outer edges of stairs not exceeding 400mm high extreme","m2",11,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Edges, risers, ends and reveals not exceeding 300mm high ","m",15,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but circular not exceeding 300mm high","m",359,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Rough formwork to soffits of:","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Slabs not exceeding 250mm thick, propping not exceeding 3,5m high","m2",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D11339*C11339","v":{"v":0,"d":"R0.00"}}]
["MASONRY","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Brickwork of clay bricks in 6:1 cement mortar","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Half brick wall circular on plan","m2",54,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["One brick wall circular on plan","m2",257,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["330mm Cavity walls formed of two half brick skins and 110mm cavity filled with concrete including wire ties","m2",212,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but circular on plan","m2",398,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Brick reinforcement ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["75mm Wide reinforcement built in horizontally ","m",14989,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150mm Wide reinforcement built in horizontally ","m",3020,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Corobrik Imperial FBX face brick, size 222 x 106 x 73mm, manufactured in accordance with 227:2007 (PC Amount of R7,500.00 per thousand bricks delivered to site, excluding VAT) pointed with flush horizontal and vertical joints ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over brickwork for face brickwork","m2",481,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Brick-on-edge header course copings, sills, etc. of face bricks pointed with recessed joints on all exposed faces","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["220mm Copings circular on plan on top of one brick walls","m",33,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["330mm Copings on top of 330 brick walls","m",92,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto. but circular on plan","m",142,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Bagging and sealing the outer face with 1:6 cement and sand mixture to receive bitumen emulsion waterproofing coating (elsewhere measured)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["To cavity walls ","m2",679,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Apply two coats of bitumen emulsion waterproofing coating","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["To cavity walls ","m2",679,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Apply two coats ABE dura.flex cementitious flexible waterproofing slurry or similar approved on concrete retaining walls application in strict accordance with manufacturer's specifications","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On retaining walls","m2",407,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["One coat 1:6 cement plaster on brickwork with steel trowel (Ref. C5) ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On external walls","m2",62,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On external circular walls","m2",205,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On external narrow widths","m2",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Prepare surfaces and remove all loose material and rinse.  Surfaces to be dry, sound and clean and cured for stipulated 28 or 14 days as stated with a moisture content, measured with a Doser Hygrometer of BD 2 scale - 8%.  Apply with one coat unreduced 100% pure acrylic emulsion water based Versus primer with two coats 100% pure acrylic water based Versus Aqua Ripple paint enhanced with marble aggregate, fillers and fungicides or similar approved.  All to manufacturer’s detailed specifications. TVOC limits (g/L of product) to be compliant to TVOC limits in Table IEQ13.1 for Green Star PEB - Custom Healthcare. Colour to Architect’s selection (Ref. C5)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On external walls","m2",269,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Movement joints, etc.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["12mm Jointex  in vertical joint built in vertically between brick walls","m2",7,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Drainage system","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100mm Diameter PVC pipe, 330mm long, through planter wall, forming band drains","No",11,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PAVING","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D11403*C11403","v":{"v":0,"d":"R0.00"}}]
["Precast concrete block paving","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["60mm Thick grey interlocking concrete paving blocks, laid in stretcher bond on a 20mm thick river sand bedding (elsewhere measured) including cement and sand filling to joints and vibrating, to walkways areas","m2",1496,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over 60mm Thick grey interlocking concrete paving for brick-on-edge header course band laid on a 250 x 75mm thick 20/13 MPa concrete base with grouted joints","m",39,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but circular on plan","m",18,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Circular cutting","m",258,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["20mm River sand ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Under  pavers","m2",1496,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Soil insecticide in accordance with SANS 5859","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Under paving etc including forming and poisoning shallow furrows, etc.","m2",1496,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["METALWORK","H1",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["BALUSTRADES","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Stainless steel balustrade overall height 931mm high, consisting of 50mm diameter  x 1.5mm thick stainless steel handrail and 25mm Diameter x 1.5mm thick stainless steel pipe as toprail and 25mm Diameter x 1.5mm thick stainless steel pipe as bottom rail, with 38 x 1.5mm stainless steel stanchion pipe welded to handrail with a 12mm diameter stainless steel stanchion pin, fixed to a 38mm diameter x 1.5mm thick stanchion, including eight vertical rails from 16mm diameter x 1.5mm stainless steel pipe, including 1.2mm stainless steel dome floor flange at each stanchion  ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Balustrade to ramps and retaining walls","m",30,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but circular","m",41,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Core drilling into concrete and epoxy grouting to fix balustrade posts, fixed with 1.2mm stainless steel dome floor flange to floor slab at 1.5m intervals","No",59,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over 50mm diameter pipe rail for closed end","No",18,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Exstra over for 90 degree bend","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Stainless steel balustrade overall height 931mm high, consisting of 50mm diameter  x 1.5mm thick stainless steel handrail and 25mm Diameter x 1.5mm thick stainless steel pipe as toprail and 25mm Diameter x 1.5mm thick stainless steel pipe as bottom rail, with 38 x 1.5mm stainless steel stanchion pipe welded to handrail with a 12mm diameter stainless steel stanchion pin, fixed to a 38mm diameter x 1.5mm thick stanchion, including eight vertical rails from 16mm diameter x 1.5mm stainless steel pipe, including 1.2mm stainless steel dome floor flange at each stanchion  ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Raking balustrade fixed to stairs and landings","m",31,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Core drilling into concrete and epoxy grouting to fix balustrade posts, fixed with 1.2mm stainless steel dome floor flange to floor slab at 1.5m intervals","No",26,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over 50mm diameter pipe rail for closed end","No",28,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Exstra over for 90 degree bend","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Stainless steel balustrade overall height 931mm high, consisting of 50mm diameter  x 1.5mm thick stainless steel handrail and 25mm Diameter x 1.5mm thick stainless steel pipe as toprail and 25mm Diameter x 1.5mm thick stainless steel pipe as bottom rail, with 38 x 1.5mm stainless steel stanchion pipe welded to handrail with a 12mm diameter stainless steel stanchion pin, fixed to a 38mm diameter x 1.5mm thick stanchion, including eight vertical rails from 16mm diameter x 1.5mm stainless steel pipe, including 1.2mm stainless steel dome floor flange at each stanchion  ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Balustrade to ramps and walkways","m",403,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Core drilling into concrete and epoxy grout for balustrade posts","No",269,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over for 90 degree bend","No",40,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over 50mm diameter pipe rail for closed end","No",13,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["HANDRAILS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Welded stainless steel handrail to ramps, stairs and landings etc. consisting of a 50mm Diameter 1.5mm thick stainless steel pipe including 12mm stainless steel rod  and 120 x 50 x 2.5mm thick stainless steel wall brackets fixed to wall with two 10mm rawlbolts at 1.5m intervals ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Raking handrail fixed to ramps, stairs and landings","m",204,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["120 x 50 x 2.5mm Thick stainless steel wall bracket fixed to wall, including two 10mm rawlbolts","No",136,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over for 90 degree bend","No",18,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D11467*C11467","v":{"v":0,"d":"R0.00"}}]
["Extra over 50mm diameter pipe rail for closed end","No",12,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["FINANCIAL PROVISIONS","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Provide the sum of R350 000.00 (Three Hundred and Fifty Thousand Rand) nett for Pergola structure","Item",1,{"v":350000,"d":"R350,000.00"},{"v":350000,"d":"R350,000.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for profit if required ","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for attendance ","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Provide the sum of R200 000.00 (Two Hundred Thousand Rand) nett for Decorative features to walls","Item",1,{"v":200000,"d":"R200,000.00"},{"v":200000,"d":"R200,000.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for profit if required ","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for attendance ","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["RAMPS AND STEPS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["EARTHWORKS","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavation in earth or compacted filling not exceeding 2m deep","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Reduced levels under ramps, steps, etc","m3",180,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over all excavations for carting away","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over all excavations for carting surplus excavated material ","m3",180,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Compaction of surfaces ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Scarify earth surface to a depth of 150mm, breaking down over size material and reconsolidate to 90% modified AASHTO density ","m2",601,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["G5 gravel layers supplied by the contractor compacted to 97% Mod AASHTO density in layers not exceeding 150mm ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Subbase under ramps, steps","m3",180,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["25 MPa/19 mm Reinforced concrete in","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ramps, steps, etc","m3",120,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fabric reinforcement","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Type 245 fabric reinforcement in ramps, etc.","m2",601,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Finishing top surfaces of concrete to an evenly brushed non-slip surface","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ramps,steps, etc","m2",601,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Rough formwork to sides","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Edges, risers, ends and reveals not exceeding 300mm high ","m",602,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["ELECTRICAL AND ICT SLEEVES","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: All sleeve pipes and pipe conduits to be supplied with draw wires as necessary for fixing of cables and wiring",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["uPVC sleeves laid in trenches (trenches elsewhere) ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["50mm Diameter sleeve pipes","m",348,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["75mm Diameter sleeve pipes","m",673,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110mm Diameter sleeve pipes","m",11973,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D11531*C11531","v":{"v":0,"d":"R0.00"}}]
["160mm Diameter sleeve pipes","m",1524,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["50mm Long radius bend or elbow","No",73,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["75mm Long radius bend or elbow","No",101,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110mm Long radius bend or elbow","No",413,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["160mm Long radius bend or elbow","No",167,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavate in earth and set excavated material aside for re-use as filling for:","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cable or sleeve trenches not exceeding 1m deep","m3",2511,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cable or sleeve trenches exceeding 1m and not exceeding 2m deep","m3",1299,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Provide bedding from carted on material from commercial sources including sifting and compaction to 90% MOD AASHTO density for backfilling to","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Selected granular material","m3",1068,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Provide main fill blanket from trench excavations in layers not exceeding 150mm thick, compacted to 95% MOD AASHTO density","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Selected fill material","m3",2742,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Surplus material from the excavations spread and levelled over the site as directed","m3",1068,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over excavations in 'earth' for cable or sleeve trenches in 'intermediate rock'","m3",381,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over excavations in 'earth' for cable or sleeve trenches in 'hard rock'","m3",381,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["MANHOLES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavate in earth for and build manhole formed  of one brick walls minimum 600mm high, plastered on the inside with cement plaster (5:1),  on 150mm  thick 25Mpa/19mm  mass concrete slab with 20Mpa fine mass  concrete  benching in bottom, floated smooth with falls including all necessary  bends, junctions  etc., including all necessary excavations,  pre-cast concrete cover slab with opening for cast iron cover and   frame  (measured  elsewhere)  set  in  cement mortar and sealed  in  tallow. Complete with cast iron nameplate stating \"ELECTRICAL MANHOLE\"","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Manhole size 1000 x 1000mm internally not exceeding 1m deep ","No",35,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Manhole size 1500 x 1500mm internally not exceeding 1m deep ","No",24,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Manhole size 1500 x 1500mm internally exceeding 1m and not exceeding 2m deep ","No",13,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavate in earth for and build manhole formed  of one brick walls minimum 600mm high, plastered on the inside with cement plaster (5:1),  on 150mm  thick 25Mpa/19mm  mass concrete slab with 20Mpa fine mass  concrete  benching in bottom, floated smooth with falls including all necessary  bends, junctions  etc., including all necessary excavations,  pre-cast concrete cover slab with opening for cast iron cover and   frame  (measured  elsewhere)  set  in  cement mortar and sealed  in  tallow. Complete with cast iron nameplate stating \"TELEPHONE AND DATA MANHOLE\"  ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Manhole size 1000 x 1000mm internally not exceeding 1m deep ","No",28,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Manhole covers, etc.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["1000 x 1000mm heavy duty SABS Type 9A cast iron single seal manhole cover and frame bedded in cement mortar","No",72,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["600mm Diameter light duty SABS Type 9A cast iron single seal manhole cover and frame bedded in cement mortar","No",28,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["HELIPAD AND STEEL BRIDGE","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["EXCAVATIONS, ETC.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavation in earth or compacted filling not exceeding 2m deep","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Concrete base","m3",115,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over excavations in earth for excavation in","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Soft rock","m3",12,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Hard rock","m3",55,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D11595*C11595","v":{"v":0,"d":"R0.00"}}]
["Extra over all excavations for carting away","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Surplus material from excavations to a dumping site to be located by the contractor","m3",96,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Risk of collapse of excavations","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sides of trench and hole excavations exceeding 1,5m and not exceeding 2.5m deep","m2",58,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Approved G7 filling supplied and carted on by the Contractor, compacted in layers not exceeding 150mm to 97% Mod. AASHTO density","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Backfilling to sides of bases","m3",19,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["UNREINFORCED CONCRETE CAST AGAINST EXCAVATED SURFACES ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["MASS CONCRETE","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["15MPa/19mm concrete","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blinding under concrete base","m3",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["REINFORCED CONCRETE CAST AGAINST EXCAVATED SURFACES ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["35 MPa/19 mm concrete in","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Concrete base","m3",96,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Concrete floor slabs","m3",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Concrete roof slab","m3",110,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Concrete intermediary slab","m3",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Circular shaped helipad walls","m3",293,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TEST BLOCKS","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Making and testing set of three 150 x 150 x 150 mm strength test cubes","No",25,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SMOOTH FORMWORK TO HELIPAD (DEGREE OF ACCURACY I)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["4000mm Diameter helipad base not exceeding 300mm high","m",13,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["4000mm Diameter conical structure 13000mm high (external diameter)","m2",163,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["3500mm Diameter conical structure 13000mm high (internal diameter)","m2",143,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["12000mm Diameter conical structure 10000mm high (external diameter)","m2",377,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["8000mm Diameter conical structure 10000mm high (internal diameter)","m2",251,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["ROUGH FORMWORKS TO SOFFITS","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Concrete slabs exceeding 250mm thick and not exceeding 500mm thick, propping 7m high","m2",7,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Concrete slabs exceeding 250mm thick and not exceeding 500mm thick, propping 13m high","m2",10,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Concrete roof slabs exceeding 250mm thick and not exceeding 500mm thick, propping 18m high","m2",314,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["REINFORCEMENT","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Mild steel reinforcement ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["10mm Diameter bars","t",7.62,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D11659*C11659","v":{"v":0,"d":"R0.00"}}]
["High tensile steel rod reinforcement to structural concrete work","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["10mm Diameter bars","t",19.05,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["12mm Diameter bars","t",26.67,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["16mm Diameter bars","t",22.86,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["WATERPROOFING","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sikalastic®-560 waterproofing membrane installed in accordance with the manufacturer`s specifications. (Sika 051 430 0333)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On flat roofs to falls","m2",314,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PAINTWORK","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Prepare surfaces and remove all loose material and rinse.  Surfaces to be dry, sound and clean and cured for stipulated 28 or 14 days as stated with a moisture content, measured with a Doser Hygrometer of BD 2 scale - 8%.  Apply with one coat unreduced 100% pure acrylic emulsion water based Versus primer with two coats 100% pure acrylic water based Versus Aqua Ripple paint enhanced with marble aggregate, fillers and fungicides or similar approved.  All to manufacturer’s detailed specifications. TVOC limits (g/L of product) to be compliant to TVOC limits in Table IEQ13.1 for Green Star PEB - Custom Healthcare. Colour to Architect’s selection (Ref. C5)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On concrete walls","m2",540,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["STEEL BRIDGE","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Mild steel","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["I sections, IPE sections, etc. in tie beams, rafters, struts, bracing, etc. in steel bridge","t",3.04,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Square and rectangular hollow section in steel bridge","t",1.52,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Angle sections, flat sections, etc. in brackets, base plates,  connector plates, etc. ","t",0.51,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["WIND SOCK, SIGNAGE, ETC.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow the amount of R 45,000.00 (Fourty Five Thousand Rand) for windsocks and signage","Item",1,{"v":45000,"d":"R45,000.00"},{"v":45000,"d":"R45,000.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for profit if required ","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for attendance ","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["THE FOLLOWING IN SERVICE TUNNEL ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Selected crushed material  from the stock piles,  to comply with the minimum specification of G7 and compacted in layers not exceeding 150mm to 95%  modified AASHTO ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Back filling  to service tunnel","m3",1195,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["30MPa/19mm concrete","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Culvert bases","m3",274,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["15MPa/19mm concrete","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blinding under culvert bases","m3",55,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Mild steel rod reinforcement to structural concrete ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["8mm Diameter bars","t",6.86,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["High tensile steel rod reinforcement to structural concrete ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["10mm Diameter bars","t",6.86,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["12mm Diameter bars","t",6.86,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["16mm Diameter bars","t",6.86,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D11723*C11723","v":{"v":0,"d":"R0.00"}}]
["20mm Diameter bars","t",6.86,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sikaguard 905 waterproofing in accordance with the manufacturer`s specifications. (Sika 051 430 0333) as per detail drawing HDG - TYP-042-036 or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Waterproofing spayed to culvert sides ","m2",2591,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Precast Concrete ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["2100 x 2100mm Class 100S precast rectangular portal culvert as per SANS 986 ","m",305,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TOTAL GENERAL SITE WORKS, ROADS AND PAVING ",null,0,null,{"$f":"SUM(E10477:E11733)","v":{"v":595000,"d":"595,000.00"}}]
[null,null,0,null,{"v":0,"d":"R0.00"}]
["SECTION 4","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["EXTERNAL WORKS (PROVISIONAL)","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["BILL NO 3","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["YARD WALLS, FENCING, ETC","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PREAMBLES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Preambles for Trades as defined in Scope of Work (C3.1 Item 4.1 & Item 4.2)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TRADE NAMES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Any reference to trade names  in the Bills of Quantities or Architect's specification or drawings shall deem to mean \"or similar and approved\"",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["THE FOLLOWING IN WALLS, ENTRANCE WALLS, ETC","H1",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 104 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["EXCAVATION, FILLING, ETC","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavation in earth or compacted filling not exceeding 2m deep","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Trenches","m3",134,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over trench and hole excavations in earth for excavation in","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Soft rock","m3",13,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Hard rock","m3",7,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over all excavations for carting away","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Surplus material from excavations and/or stock piles on site to a dumping site to be located by the contractor","m3",73,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Risk of collapse of excavations","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sides of trench and hole excavations not exceeding 1,5m deep","m2",384,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Selected earth filling obtained from the excavations and/or prescribed stock piles on site in layers of 150mm thick compacted to 93% Mod AASHTO density","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Backfilling to trenches, holes, etc","m3",61,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["CONCRETE","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 110 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["UNREINFORCED CONCRETE CAST AGAINST EXCAVATED SURFACES ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["15MPa/19mm mass concrete","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D11787*C11787","v":{"v":0,"d":"R0.00"}}]
["Surface blindings under footings and bases","m3",9,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["25MPa/19mm mass concrete","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Strip footings","m3",45,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["BRICKWORK","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 116 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Brickwork of clay bricks in 6:1 cement mortar","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Brick piers","m3",7,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["One brick walls in foundations","m2",128,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["One brick walls","m2",169,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Brick reinforcement","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150mm Wide reinforcement built in horizontally","m",2430,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 142 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["EXTERNAL PLASTER","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["One coat 1:6 cement plaster on brickwork","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On exterior walls","m2",406,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On narrow widths","m2",89,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 152 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["ON FLOATED PLASTER","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Prepare surfaces and remove all loose material and rinse.  Surfaces to be dry, sound and clean and cured for stipulated 28 or 14 days as stated with a moisture content, measured with a Doser Hygrometer of BD 2 scale - 8%.  Apply with one coat unreduced 100% pure acrylic emulsion water based Versus primer with two coats 100% pure acrylic water based Versus Aqua Ripple paint enhanced with marble aggregate, fillers and fungicides or similar approved.  All to manufacturer’s detailed specifications. TVOC limits (g/L of product) to be compliant to TVOC limits in Table IEQ13.1 for Green Star PEB - Custom Healthcare. Colour to Architect’s selection (Ref. C5)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["On external walls","m2",495,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["FENCING","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 136 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Wirewall fencing systems or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for clearing site for the width of 1 000 mm where fencing runs are to be erected including removing trees, shrubs etc. not exceeding 200 mm girth, grubbing up roots and roughly levelling","m",4450,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["3000mm long Securemax post in zinc aluminium coated material (MPA 400 to 420), with a 2450mm long roll formed full panel height clamp (referred to as cover plate) in Zinc aluminium material (MPA 400 to 420). All fixings, 5 x 100mm long tie rods, 5 x fixing cleats, 5 x washers and 5 x sheer nuts per post shall be manufactured from 304 stainless steel grade. Post to be complete with UPVC end cap. Post and cover plate shall have a Ferrro Vedoc VP Black grey powder coated finish (RAL 7021). Post to be embedded in 400 x 400 x 600 mm mass concrete (15 MPa) base including excavations and backfilling","No",1459,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allview 3510 panel size 3050 x 2400mm high, with 3mm on 4mm high tensile zinc aluminium coated wire with aperture size (centres) @ 75mm x 12.7mm. Panel to be reinforced with 4 x 40 x 113mm deep V formations horizontal recessed bends for rigidity. Panel has double vertical lines that is pinned from top to bottom into post and secured with a full panel height roll formed clamp. All fixtures are at the back of the post in recess. Panel is guaranteed to sit flush with post line as it is clamped within post. Post has no climbing points to assist climbing. Panel to be Ferro Vedoc VP Black grey Powder coated finish (RAL 7021). Panel to include spike rails fixed to the top of the panel by means of anti-tampering stainless steel grade 304 fixings at 150mm intervals. Spike finish shall be Ferro Vedoc VP Black grey Powder coated finish (RAL 7021)","No",957,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Securemax 50 panel size 3050 x 2400mm high, with 3mm on 4mm high tensile zinc aluminium coated wire with aperture size (centres) @ 75mm x 50mm. Panel to be reinforced with 4 x 40 x 113mm deep V formations horizontal recessed bends for rigidity. Panel has double vertical lines that is pinned from top to bottom into post and secured with a full panel height roll formed clamp. All fixtures are at the back of the post in recess. Panel is guaranteed to sit flush with post line as it is clamped within post. Post has no climbing points to assist climbing. Panel to be Ferro Vedoc VP Black grey Powder coated finish (RAL 7021). Panel to include spike rails fixed to the top of the panel by means of anti-tampering stainless steel grade 304 fixings at 150mm intervals. Spike finish shall be Ferro Vedoc VP Black grey Powder coated finish (RAL 7021)","No",502,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allview 3510 panel underdig size 3050 x 400mm high, with 3mm on 4mm high tensile zinc aluminium coated wire with aperture size (centres) @ 75mm x 12.7mm. Panel to be flat with no V formations horizontal recessed bends. Panel is installed in the ground before concrete hardens between the Securemax post below the above ground fence panel. Panel has double vertical lines that is pinned into post. Panel will be in Zinc aluminium coated finish","No",957,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Securemax 50 panel underdig size 3050 x 400mm high, with 3mm on 4mm high tensile zinc aluminium coated wire with aperture size (centres) @ 75mm x 50mm. Panel to be flat with no V formations horizontal recessed bends. Panel is installed in the ground before concrete hardens between the Securemax post below the above ground fence panel. Panel has double vertical lines that is pinned into post. Panel will be in Zinc aluminium coated finish","No",502,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavations not exceeding 2m deep for underdig","m3",712,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Wirewall Securemax fencing fixed to top of retaining wall or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["1500mm long Securemax intermediate post in zinc aluminium coated material (MPA 400 to 420), with a 1500mm long roll formed full panel height clamp (referred to as cover plate) in Zinc aluminium material (MPA 400 to 420). All fixings, 3 x 100mm long tie rods, 3 x fixing cleats, 3 x washers and 3 x sheer nuts per post shall be manufactured from 304 stainless steel grade. Post to be complete with UPVC end cap. Post and cover plate shall have a Ferrro Vedoc VP Black grey powder coated finish (RAL 7021). Post to be fixed to 150 x 150 x 8mm with a 300mm upright rolled formed section in 3mm material welded to the base plate. Post slides over base plate and fixed at two fixing points to the upright  with 1 x 31mm tie rod, 1 x fixing cleat, 1 x washer and 1 x shear nut per base plate supplied. Base plate to be mild steel with Plascoat PPA571 Grey 642 coating","No",131,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D11851*C11851","v":{"v":0,"d":"R0.00"}}]
["1500mm long Securemax corner post in zinc aluminium coated material (MPA 400 to 420), with a 1500mm long roll formed full panel height clamp (referred to as cover plate) in Zinc aluminium material (MPA 400 to 420). All fixings, 3 x 100mm long tie rods, 3 x fixing cleats, 3 x washers and 3 x sheer nuts per post shall be manufactured from 304 stainless steel grade. Post to be complete with UPVC end cap. Post and cover plate shall have a Ferrro Vedoc VP Black grey powder coated finish (RAL 7021). Post to be fixed to 200 x 150 x 8mm with a 300mm upright rolled formed section in 3mm material welded to the base plate. Post slides over base plate and fixed at two fixing points to the upright  with 1 x 31mm tie rod, 1 x fixing cleat, 1 x washer and 1 x shear nut per base plate supplied. Base plate to be mild steel with Plascoat PPA571 Grey 642 coating","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allview 3510 panel size 3050 x 1500mm high, with 3mm on 4mm high tensile zinc aluminium coated wire with aperture size (centres) @ 75mm x 12.7mm. Panel to be reinforced with 2 x 40 x 113mm deep V formations horizontal recessed bends for rigidity. Panel has double vertical lines that is pinned from top to bottom into post and secured with a full panel height roll formed clamp. All fixtures are at the back of the post in recess. Panel is guaranteed to sit flush with post line as it is clamped within post. Post has no climbing points to assist climbing. Panel to be Ferro Vedoc VP Black grey Powder coated finish (RAL 7021). Panel to include spike rails fixed to the top of the panel by means of anti-tampering stainless steel grade 304 fixings at 150mm intervals. Spike finish shall be Ferro Vedoc VP Black grey Powder coated finish (RAL 7021)","No",131,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Wirewall Securemax fencing fixed to top of brick wall or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["2000mm long Securemax intermediate post in zinc aluminium coated material (MPA 400 to 420), with a 2000mm long roll formed full panel height clamp (referred to as cover plate) in Zinc aluminium material (MPA 400 to 420). All fixings, 4 x 100mm long tie rods, 4 x fixing cleats, 4 x washers and 4 x sheer nuts per post shall be manufactured from 304 stainless steel grade. Post to be complete with UPVC end cap. Post and cover plate shall have a Ferrro Vedoc VP Black grey powder coated finish (RAL 7021). Post to be fixed to 150 x 150 x 8mm with a 300mm upright rolled formed section in 3mm material welded to the base plate. Post slides over base plate and fixed at two fixing points to the upright  with 1 x 31mm tie rod, 1 x fixing cleat, 1 x washer and 1 x shear nut per base plate supplied. Base plate to be mild steel with Plascoat PPA571 Grey 642 coating","No",36,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["2000mm long Securemax corner post in zinc aluminium coated material (MPA 400 to 420), with a 2000mm long roll formed full panel height clamp (referred to as cover plate) in Zinc aluminium material (MPA 400 to 420). All fixings, 4 x 100mm long tie rods, 4 x fixing cleats, 4 x washers and 4 x sheer nuts per post shall be manufactured from 304 stainless steel grade. Post to be complete with UPVC end cap. Post and cover plate shall have a Ferrro Vedoc VP Black grey powder coated finish (RAL 7021). Post to be fixed to 200 x 150 x 8mm with a 300mm upright rolled formed section in 3mm material welded to the base plate. Post slides over base plate and fixed at two fixing points to the upright  with 1 x 31mm tie rod, 1 x fixing cleat, 1 x washer and 1 x shear nut per base plate supplied. Base plate to be mild steel with Plascoat PPA571 Grey 642 coating","No",9,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Securemax 50 panel size 3050 x 2000mm high, with 3mm on 4mm high tensile zinc aluminium coated wire with aperture size (centres) @ 75mm x 50mm. Panel to be reinforced with 3 x 40 x 113mm deep V formations horizontal recessed bends for rigidity. Panel has double vertical lines that is pinned from top to bottom into post and secured with a full panel height roll formed clamp. All fixtures are at the back of the post in recess. Panel is guaranteed to sit flush with post line as it is clamped within post. Post has no climbing points to assist climbing. Panel to be Ferro Vedoc VP Black grey Powder coated finish (RAL 7021). Panel to include spike rails fixed to the top of the panel by means of anti-tampering stainless steel grade 304 fixings at 150mm intervals. Spike finish shall be Ferro Vedoc VP Black grey Powder coated finish (RAL 7021)","No",36,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Wirewall fencing fixed inbetween brickwork or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["1500mm long Securemax post in zinc aluminium coated material (MPA 400 to 420), with a 1500mm long roll formed full panel height clamp (referred to as cover plate) in Zinc aluminium material (MPA 400 to 420). All fixings, 3 x 100mm long tie rods, 3 x fixing cleats, 3 x washers and 3 x sheer nuts per post shall be manufactured from 304 stainless steel grade. Post to be complete with UPVC end cap. Post and cover plate shall have a Ferrro Vedoc VP Black grey powder coated finish (RAL 7021). Post to be fixed to wall by drilling slots into posts on site on one side of post and fixed to brick work with chemical anchors at 150mm intervals ","No",48,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allview 3510 panel size 3050 x 1500mm high, with 3mm on 4mm high tensile zinc aluminium coated wire with aperture size (centres) @ 75mm x 12.7mm. Panel to be reinforced with 2 x 40 x 113mm deep V formations horizontal recessed bends for rigidity. Panel has double vertical lines that is pinned from top to bottom into post and secured with a full panel height roll formed clamp. All fixtures are at the back of the post in recess. Panel is guaranteed to sit flush with post line as it is clamped within post. Post has no climbing points to assist climbing. Panel to be Ferro Vedoc VP Black grey Powder coated finish (RAL 7021). Panel to include spike rails fixed to the top of the panel by means of anti-tampering stainless steel grade 304 fixings at 150mm intervals. Spike finish shall be Ferro Vedoc VP Black grey Powder coated finish (RAL 7021)","No",48,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Wirewall pedestrian gates or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Securemex 50 security fence pedestrian single gate, size 1200mm wide x 2400mm high, in single leave formed of 50 x 2.8mm tubular frames with bracing complete with two hinges, eye bolt, bolts and barrel bolt. Frame covered with with 3mm on 4mm high tensile zinc aluminium coated wire with aperture size (centres) @ 75mm x 50mm. Panel to be reinforced with 4 x 40 x 113mm deep V formations horizontal recessed bends for rigidity and including 500 mm long approved chain spot welded to gate and union padlock No 3122 with two 100 x 3mm galvanised corner posts with 300 x 300 x 6mm base plate cast in 450 x 450 x 900mm concrete base","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Securemex 50 security fence pedestrian single gate, size 1500mm wide x 2000mm high, in single leave formed of 50 x 2.8mm tubular frames with bracing complete with two hinges, eye bolt, bolts and barrel bolt. Frame covered with with 3mm on 4mm high tensile zinc aluminium coated wire with aperture size (centres) @ 75mm x 50mm. Panel to be reinforced with 4 x 40 x 113mm deep V formations horizontal recessed bends for rigidity and including 500 mm long approved chain spot welded to gate and union padlock No 3122 with two 100 x 3mm galvanised corner posts with 300 x 300 x 6mm base plate cast in 450 x 450 x 900mm concrete base","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Securemex 50 security fence pedestrian double gate, size 2000mm wide x 2400mm high, in equal leaves each leaf formed of 50 x 2.8mm tubular frames with bracing complete with four hinges, eye bolts, bolts and barrel bolt. Frame covered with with 3mm on 4mm high tensile zinc aluminium coated wire with aperture size (centres) @ 75mm x 50mm. Panel to be reinforced with 4 x 40 x 113mm deep V formations horizontal recessed bends for rigidity and including 500 mm long approved chain spot welded to gate and union padlock No 3122 with two 100 x 3mm galvanised corner posts with 300 x 300 x 6mm base plate cast in 450 x 450 x 900mm concrete and 50 x 3mm galvanised straining posts with 300 x 300 x 6mm base plate cast in 450 x 760 x 600mm concrete base","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allview 3510 security fence padestrian double gate, size 4000mm wide x 2400mm high, in equal leaves each leaf formed of 50 x 2.8mm tubular frames with bracing complete with four hinges, eye bolts, bolts and barrel bolt. Frame covered with 3mm on 4mm high tensile zinc aluminium coated wire with aperture size (centres) @ 75mm x 12.7mm. Panel to be reinforced with 4 x 40 x 113mm deep V formations horizontal recessed bends for rigidity and including 500 mm long approved chain spot welded to gate and union padlock No 3122 with two 100 x 3mm galvanised corner posts with 300 x 300 x 6mm base plate cast in 450 x 450 x 900mm concrete and 50 x 3mm galvanised straining posts with 300 x 300 x 6mm base plate cast in 450 x 760 x 600mm concrete base","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Wirewall double gates or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Securemex 50 security fence double gate, size 2000mm wide x 2400mm high, in equal leaves each leaf formed of 50 x 2.8mm tubular frames with bracing complete with four hinges, eye bolts, bolts and barrel bolt. Frame covered with with 3mm on 4mm high tensile zinc aluminium coated wire with aperture size (centres) @ 75mm x 50mm. Panel to be reinforced with 4 x 40 x 113mm deep V formations horizontal recessed bends for rigidity and including 500 mm long approved chain spot welded to gate and union padlock No 3122 with two 100 x 3mm galvanised corner posts with 300 x 300 x 6mm base plate cast in 450 x 450 x 900mm concrete and 50 x 3mm galvanised straining posts with 300 x 300 x 6mm base plate cast in 450 x 760 x 600mm concrete base","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allview 3510 security fence double gate, size 2500mm wide x 2400mm high, in equal leaves each leaf formed of 50 x 2.8mm tubular frames with bracing complete with four hinges, eye bolts, bolts and barrel bolt. Frame covered with 3mm on 4mm high tensile zinc aluminium coated wire with aperture size (centres) @ 75mm x 12.7mm. Panel to be reinforced with 4 x 40 x 113mm deep V formations horizontal recessed bends for rigidity and including 500 mm long approved chain spot welded to gate and union padlock No 3122 with two 100 x 3mm galvanised corner posts with 300 x 300 x 6mm base plate cast in 450 x 450 x 900mm concrete and 50 x 3mm galvanised straining posts with 300 x 300 x 6mm base plate cast in 450 x 760 x 600mm concrete base","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Securemex 50 security fence double gate, size 2500mm wide x 2400mm high, in equal leaves each leaf formed of 50 x 2.8mm tubular frames with bracing complete with four hinges, eye bolts, bolts and barrel bolt. Frame covered with with 3mm on 4mm high tensile zinc aluminium coated wire with aperture size (centres) @ 75mm x 50mm. Panel to be reinforced with 4 x 40 x 113mm deep V formations horizontal recessed bends for rigidity and including 500 mm long approved chain spot welded to gate and union padlock No 3122 with two 100 x 3mm galvanised corner posts with 300 x 300 x 6mm base plate cast in 450 x 450 x 900mm concrete and 50 x 3mm galvanised straining posts with 300 x 300 x 6mm base plate cast in 450 x 760 x 600mm concrete base","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Securemex 50 security fence double gate, size 3000mm wide x 2400mm high, in equal leaves each leaf formed of 50 x 2.8mm tubular frames with bracing complete with four hinges, eye bolts, bolts and barrel bolt. Frame covered with with 3mm on 4mm high tensile zinc aluminium coated wire with aperture size (centres) @ 75mm x 50mm. Panel to be reinforced with 4 x 40 x 113mm deep V formations horizontal recessed bends for rigidity and including 500 mm long approved chain spot welded to gate and union padlock No 3122 with two 100 x 3mm galvanised corner posts with 300 x 300 x 6mm base plate cast in 450 x 450 x 900mm concrete and 50 x 3mm galvanised straining posts with 300 x 300 x 6mm base plate cast in 450 x 760 x 600mm concrete base","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allview 3510 security fence double gate, size 3500mm wide x 2400mm high, in equal leaves each leaf formed of 50 x 2.8mm tubular frames with bracing complete with four hinges, eye bolts, bolts and barrel bolt. Frame covered with 3mm on 4mm high tensile zinc aluminium coated wire with aperture size (centres) @ 75mm x 12.7mm. Panel to be reinforced with 4 x 40 x 113mm deep V formations horizontal recessed bends for rigidity and including 500 mm long approved chain spot welded to gate and union padlock No 3122 with two 100 x 3mm galvanised corner posts with 300 x 300 x 6mm base plate cast in 450 x 450 x 900mm concrete and 50 x 3mm galvanised straining posts with 300 x 300 x 6mm base plate cast in 450 x 760 x 600mm concrete base","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Securemex 50 security fence double gate, size 4000mm wide x 2000mm high, in equal leaves each leaf formed of 50 x 2.8mm tubular frames with bracing complete with four hinges, eye bolts, bolts and barrel bolt. Frame covered with with 3mm on 4mm high tensile zinc aluminium coated wire with aperture size (centres) @ 75mm x 50mm. Panel to be reinforced with 4 x 40 x 113mm deep V formations horizontal recessed bends for rigidity and including 500 mm long approved chain spot welded to gate and union padlock No 3122 with two 100 x 3mm galvanised corner posts with 300 x 300 x 6mm base plate cast in 450 x 450 x 900mm concrete and 50 x 3mm galvanised straining posts with 300 x 300 x 6mm base plate cast in 450 x 760 x 600mm concrete base","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allview 3510 security fence double gate, size 4000mm wide x 2400mm high, in equal leaves each leaf formed of 50 x 2.8mm tubular frames with bracing complete with four hinges, eye bolts, bolts and barrel bolt. Frame covered with 3mm on 4mm high tensile zinc aluminium coated wire with aperture size (centres) @ 75mm x 12.7mm. Panel to be reinforced with 4 x 40 x 113mm deep V formations horizontal recessed bends for rigidity and including 500 mm long approved chain spot welded to gate and union padlock No 3122 with two 100 x 3mm galvanised corner posts with 300 x 300 x 6mm base plate cast in 450 x 450 x 900mm concrete and 50 x 3mm galvanised straining posts with 300 x 300 x 6mm base plate cast in 450 x 760 x 600mm concrete base","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allview 3510 security fence double gate, size 4500mm wide x 2400mm high, in equal leaves each leaf formed of 50 x 2.8mm tubular frames with bracing complete with four hinges, eye bolts, bolts and barrel bolt. Frame covered with 3mm on 4mm high tensile zinc aluminium coated wire with aperture size (centres) @ 75mm x 12.7mm. Panel to be reinforced with 4 x 40 x 113mm deep V formations horizontal recessed bends for rigidity and including 500 mm long approved chain spot welded to gate and union padlock No 3122 with two 100 x 3mm galvanised corner posts with 300 x 300 x 6mm base plate cast in 450 x 450 x 900mm concrete and 50 x 3mm galvanised straining posts with 300 x 300 x 6mm base plate cast in 450 x 760 x 600mm concrete base","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allview 3510 security fence double gate, size 5000mm wide x 2400mm high, in equal leaves each leaf formed of 50 x 2.8mm tubular frames with bracing complete with four hinges, eye bolts, bolts and barrel bolt. Frame covered with 3mm on 4mm high tensile zinc aluminium coated wire with aperture size (centres) @ 75mm x 12.7mm. Panel to be reinforced with 4 x 40 x 113mm deep V formations horizontal recessed bends for rigidity and including 500 mm long approved chain spot welded to gate and union padlock No 3122 with two 100 x 3mm galvanised corner posts with 300 x 300 x 6mm base plate cast in 450 x 450 x 900mm concrete and 50 x 3mm galvanised straining posts with 300 x 300 x 6mm base plate cast in 450 x 760 x 600mm concrete base","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Securemex 50 security fence double gate, size 5500mm wide x 2400mm high, in equal leaves each leaf formed of 50 x 2.8mm tubular frames with bracing complete with four hinges, eye bolts, bolts and barrel bolt. Frame covered with with 3mm on 4mm high tensile zinc aluminium coated wire with aperture size (centres) @ 75mm x 50mm. Panel to be reinforced with 4 x 40 x 113mm deep V formations horizontal recessed bends for rigidity and including 500 mm long approved chain spot welded to gate and union padlock No 3122 with two 100 x 3mm galvanised corner posts with 300 x 300 x 6mm base plate cast in 450 x 450 x 900mm concrete and 50 x 3mm galvanised straining posts with 300 x 300 x 6mm base plate cast in 450 x 760 x 600mm concrete base","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allview 3510 security fence double gate, size 6000mm wide x 2400mm high, in equal leaves each leaf formed of 50 x 2.8mm tubular frames with bracing complete with four hinges, eye bolts, bolts and barrel bolt. Frame covered with 3mm on 4mm high tensile zinc aluminium coated wire with aperture size (centres) @ 75mm x 12.7mm. Panel to be reinforced with 4 x 40 x 113mm deep V formations horizontal recessed bends for rigidity and including 500 mm long approved chain spot welded to gate and union padlock No 3122 with two 100 x 3mm galvanised corner posts with 300 x 300 x 6mm base plate cast in 450 x 450 x 900mm concrete and 50 x 3mm galvanised straining posts with 300 x 300 x 6mm base plate cast in 450 x 760 x 600mm concrete base","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Securemex 50 security fence double gate, size 6000mm wide x 2400mm high, in equal leaves each leaf formed of 50 x 2.8mm tubular frames with bracing complete with four hinges, eye bolts, bolts and barrel bolt. Frame covered with with 3mm on 4mm high tensile zinc aluminium coated wire with aperture size (centres) @ 75mm x 50mm. Panel to be reinforced with 4 x 40 x 113mm deep V formations horizontal recessed bends for rigidity and including 500 mm long approved chain spot welded to gate and union padlock No 3122 with two 100 x 3mm galvanised corner posts with 300 x 300 x 6mm base plate cast in 450 x 450 x 900mm concrete and 50 x 3mm galvanised straining posts with 300 x 300 x 6mm base plate cast in 450 x 760 x 600mm concrete base","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allview 3510 security fence double gate, size 7000mm wide x 2400mm high, in equal leaves each leaf formed of 50 x 2.8mm tubular frames with bracing complete with four hinges, eye bolts, bolts and barrel bolt. Frame covered with 3mm on 4mm high tensile zinc aluminium coated wire with aperture size (centres) @ 75mm x 12.7mm. Panel to be reinforced with 4 x 40 x 113mm deep V formations horizontal recessed bends for rigidity and including 500 mm long approved chain spot welded to gate and union padlock No 3122 with two 100 x 3mm galvanised corner posts with 300 x 300 x 6mm base plate cast in 450 x 450 x 900mm concrete and 50 x 3mm galvanised straining posts with 300 x 300 x 6mm base plate cast in 450 x 760 x 600mm concrete base","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Securemex 50 security fence double gate, size 7500mm wide x 2400mm high, in equal leaves each leaf formed of 50 x 2.8mm tubular frames with bracing complete with four hinges, eye bolts, bolts and barrel bolt. Frame covered with with 3mm on 4mm high tensile zinc aluminium coated wire with aperture size (centres) @ 75mm x 50mm. Panel to be reinforced with 4 x 40 x 113mm deep V formations horizontal recessed bends for rigidity and including 500 mm long approved chain spot welded to gate and union padlock No 3122 with two 100 x 3mm galvanised corner posts with 300 x 300 x 6mm base plate cast in 450 x 450 x 900mm concrete and 50 x 3mm galvanised straining posts with 300 x 300 x 6mm base plate cast in 450 x 760 x 600mm concrete base","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Wirewall sliding gates or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Securemex 50 security fence sliding gate, size 4000mm wide x 2400mm high, formed of 50 x 50 x 3mm gate frame complete with 50 x 3mm flat bar, with two 100 x 100 x 2mm gate posts with pole cap each set in 25Mpa concrete bases size 400 x 400 x 500mm high.  A 100mm high toughened steel shark tooth spike to be affixed to panel edge internally at 150mm intervals using anti-vandal bolts.  Gate to include 80mm diameter gate wheels running on track to consist of 20mm diameter mild steel roundbar track, complete with mild steel 100 x 55mm IPE section 8000m long set in 25Mpa concrete, size 8000 x 200 x 200mm wide","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allview 3510 security fence sliding gate, size 1500mm wide x 2400mm high, formed of 50 x 50 x 3mm gate frame complete with 50 x 3mm flat bar, with two 100 x 100 x 2mm gate posts with pole cap each set in 25Mpa concrete bases size 400 x 400 x 500mm high.  A 100mm high toughened steel shark tooth spike to be affixed to panel edge internally at 150mm intervals using anti-vandal bolts.  Gate to include 80mm diameter gate wheels running on track to consist of 20mm diameter mild steel roundbar track, complete with mild steel 100 x 55mm IPE section 3000m long set in 25Mpa concrete, size 3000 x 200 x 200mm wide","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D11915*C11915","v":{"v":0,"d":"R0.00"}}]
["Securemex 50 security fence sliding gate, size 4200mm wide x 2400mm high, formed of 50 x 50 x 3mm gate frame complete with 50 x 3mm flat bar, with two 100 x 100 x 2mm gate posts with pole cap each set in 25Mpa concrete bases size 400 x 400 x 500mm high.  A 100mm high toughened steel shark tooth spike to be affixed to panel edge internally at 150mm intervals using anti-vandal bolts.  Gate to include 80mm diameter gate wheels running on track to consist of 20mm diameter mild steel roundbar track, complete with mild steel 100 x 55mm IPE section 8400m long set in 25Mpa concrete, size 8400 x 200 x 200mm wide","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Securemex 50 security fence sliding gate, size 7000mm wide x 2400mm high, formed of 50 x 50 x 3mm gate frame complete with 50 x 3mm flat bar, with two 100 x 100 x 2mm gate posts with pole cap each set in 25Mpa concrete bases size 400 x 400 x 500mm high.  A 100mm high toughened steel shark tooth spike to be affixed to panel edge internally at 150mm intervals using anti-vandal bolts.  Gate to include 80mm diameter gate wheels running on track to consist of 20mm diameter mild steel roundbar track, complete with mild steel 100 x 55mm IPE section 14000m long set in 25Mpa concrete, size 14000 x 200 x 200mm wide","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Centurion Systems light industrial D10 Turbo™ 24V DC sliding gate operator, capable of handling a gate mass of 240kg - 1000kg at opening speed of 40 metres per minute with 2A 24V SM charger 2 x 7Ah battery and 2 x sets safety beams with 2 metre passive sensitive edge with anti lift cage and with P36 passive edge, complete with steel rack, including foundation plate. System to include Photon wireless infrared vehicle detection beams, installed in accordance with manufacturer`s recommendations","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Kerbing to inside of fence line","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150 x 75mm Edging kerb as SABS Specification 927 Fig.12, in approximately 1000mm lengths, bedded, jointed and pointed including unreinforced concrete foundation size 100 x 75mm thick under and 200 x 200 x 100mm high unreinforced concrete Class B haunching behind, including necessary excavation","m",2918,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over excavations in earth for excavation in","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Soft rock","m3",71,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Intermediate rock","m3",71,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Hard rock","m3",36,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TURNSTILES","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Turnstar Systems Titan 4 single high security turnstile size 1430 x 2250mm high  with rotor diameter of 1.2m and 4-arm 90 degree rotor arm configuration, bolted to 20MPa concrete slab with 7No. M12 x 75mm countersunk anchor bolts. (Supplier Tel no. 011-786 1633) or similar approved","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["VEHICLE BARRIER GATE","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Turnstar Velocity Raptor automatic industrial vehicle barrier with swiftdrive with 316 grade stainless steel cabinet with octagonal powder coated aluminium articulated barrier arm and recessed Velocity spike barrier complete with courtesy light, integrated LED light strip, diffuser and red reflective tape, combined logic and loop detector, bolted to reinforced concrete base and connected to 220V single phase power supply (electrical supply part of electrical installation) all in accordance with manufacturer's specifications (Supplier Tel no. 011 786 1633), size 3000mm wide or similar approved","No",14,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but size 4000mm wide ","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TOTAL YARD WALLS, FENCING, ETC",null,0,null,{"$f":"SUM(E11735:E11943)","v":{"v":0,"d":"0.00"}}]
[null,null,0,null,{"v":0,"d":"R0.00"}]
["SECTION 4","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["EXTERNAL WORKS (PROVISIONAL)","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["BILL NO 4","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["LANDSCAPING","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PREAMBLES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Preambles for Trades as defined in Scope of Work (C3.1 Item 4.1 & Item 4.2)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TRADE NAMES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Any reference to trade names in the Bills of Quantities or  Architect's specification or drawings shall deem to mean \"or similar and approved\"",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 154 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["WALKWAY PAVING  ","H1",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavate in earth or compacted filling not exceeding 2m deep below natural or reduced ground level  ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Reduced levels under paving etc","m3",456,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over all excavations for carting away","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over all excavations for carting surplus excavated material ","m3",456,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Compaction of surfaces ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Scarify earth surface to a depth of 150mm, breaking down over size material and reconsolidate to 90% modified AASHTO density ","m2",3037,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["G5 gravel layers supplied by the contractor compacted to 97% Mod AASHTO density in layers not exceeding 150mm ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D11979*C11979","v":{"v":0,"d":"R0.00"}}]
["Subbase under paving","m3",456,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["20mm River sand ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Under  pavers","m2",3037,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Approved weed killer (Certificate to be provided before payment)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Hyvar X or other equally approved soil herbicide at a rate of 50 gram/m2 under paving etc.","m2",3037,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Precast concrete block paving","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["60mm Thick grey interlocking concrete paving blocks, laid in stretcher bond on a 20mm thick river sand bedding (elsewhere measured) including cement and sand filling to joints and vibrating, to walkways areas","m2",1710,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over 60mm Thick grey interlocking concrete paving for rectangular paver header course band laid on a 250 x 75mm thick 20/13 MPa concrete base with grouted joints","m",920,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but circular on plan","m",721,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["60mm Thick multi-blend interlocking concrete paving blocks, laid in stretcher bond on a 20mm thick river sand bedding (elsewhere measured) including cement and sand filling to joints and vibrating, to walkways areas","m2",1327,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over 60mm Thick multi-blend interlocking concrete paving for rectangular paver header course band laid on a 250 x 75mm thick 20/13 MPa concrete base with grouted joints","m",722,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but circular on plan","m",141,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Circular cutting","m",861,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Header coarse to planter edges","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["50mm Thick Tuscan blend Clay paving bricks Header coarse laid on a 250 x 75mm thick 20/13MPa concrete footing with grouted joints","m",422,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but circular on plan","m",297,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["IN-SITU CONCRETE PAVING, ETC","H1",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavate in earth or compacted filling not exceeding 2m deep below natural or reduced ground level  ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Reduced levels under pavings, etc","m3",1223,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over all excavations for carting away","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over all excavations for carting surplus excavated material and spreading, levelling and lightly compacting on site where directed average 500m from the excavations (Measured nett- no allowance made for bulking)","m3",1223,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Compaction of surfaces ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Scarify earth surface to a depth of 150mm, breaking down over size material and reconsolidate to 93% modified AASHTO density ","m2",8152,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["G5 gravel layers supplied by the contractor compacted to 97% Mod AASHTO density in layers not exceeding 150mm ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Subbase under concrete paving","m3",1223,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Mass concrete (20Mpa) with 13mm \"Yellow & black\" stone from Lafarge (sample to be approved) cast in panels in:","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Concrete paving","m3",501,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Mass concrete (20Mpa) with 13-19mm ornamental aggregate (10% black stone in Ferro mix from Afrisam) cast in panels in:","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Concrete paving","m3",558,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sandblasting of concrete surfaces to expose aggregate","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sandblast concrete paving","m2",8152,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Finishing top surfaces of concrete to an evenly brushed non-slip surface","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D12043*C12043","v":{"v":0,"d":"R0.00"}}]
["Paving","m2",8152,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["General Formwork","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Edges, risers, ends and reveals not exceeding 300mm high or wide","m",3799,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but circular on plan","m",663,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["10mm Jointex or other approved cane fibre filler board in expansion joint between edge of concrete paving and walls in narrow widths not exceeding 150mm wide including tacking to face of wall and polysulphide sealant between concrete and brickwork","m",3090,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Movement joints","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["3 x 40mm Saw cut joints in top of concrete surface bed ","m",2659,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fabric reinforcement","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Type 193 fabric reinforcement in concrete surface beds, slabs, etc. ","m2",8152,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["One layer of 250 micron green polyethylene waterproof sheeting sealed at laps with PVC self adhesive tape","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Under aprons, paving, steps, ramps","m2",8152,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["IN-SITU CONCRETE TO LOADING PLATFORMS, ETC","H1",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavate in earth or compacted filling not exceeding 2m deep below natural or reduced ground level  ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Reduced levels under concrete surface bed","m3",67,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over all excavations for carting away","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over all excavations for carting surplus excavated material and spreading, levelling and lightly compacting on site where directed average 500m from the excavations (Measured nett- no allowance made for bulking)","m3",67,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Compaction of surfaces ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Scarify earth surface to a depth of 150mm, breaking down over size material and reconsolidate to 93% modified AASHTO density ","m2",444,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["G5 gravel layers supplied by the contractor compacted to 97% Mod AASHTO density in layers not exceeding 150mm","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Subbase under concrete surface bed","m3",67,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Mass concrete (30Mpa) cast in panels in:","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Concrete surface bed","m3",58,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Finishing top surfaces of concrete to an evenly brushed non-slip surface","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Concrete surface bed","m2",444,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["General Formwork","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Edges, risers, ends and reveals not exceeding 300mm high or wide","m",92,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but circular on plan","m",8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["10mm Jointex or other approved cane fibre filler board in expansion joint between edge of concrete paving and walls in narrow widths not exceeding 150mm wide including tacking to face of wall and polysulphide sealant between concrete and brickwork","m",94,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Movement joints","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["3 x 40mm Saw cut joints in top of concrete surface bed ","m",64,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fabric reinforcement","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Type 193 fabric reinforcement in concrete surface bed ","m2",444,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D12107*C12107","v":{"v":0,"d":"R0.00"}}]
["One layer of 250 micron green polyethylene waterproof sheeting sealed at laps with PVC self adhesive tape","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Under aprons","m2",444,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["IN-SITU CONCRETE APRONS, ETC","H1",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavate in earth or compacted filling not exceeding 2m deep below natural or reduced ground level  ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Reduced levels under aprons","m3",311,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over all excavations for carting away","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over all excavations for carting surplus excavated material and spreading, levelling and lightly compacting on site where directed average 500m from the excavations (Measured nett- no allowance made for bulking)","m3",311,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Compaction of surfaces ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Scarify earth surface to a depth of 150mm, breaking down over size material and reconsolidate to 93% modified AASHTO density ","m2",2389,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["G5 gravel layers supplied by the contractor compacted to 97% Mod AASHTO density in layers not exceeding 150mm","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Subbase under apron ","m3",311,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Mass concrete (30Mpa) cast in panels in:","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Aprons","m3",239,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Finishing top surfaces of concrete to an evenly brushed non-slip surface","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Aprons","m2",2389,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["General Formwork","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Edges, risers, ends and reveals not exceeding 300mm high or wide","m",1351,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but circular on plan","m",26,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["10mm Jointex or other approved cane fibre filler board in expansion joint between edge of concrete paving and walls in narrow widths not exceeding 150mm wide including tacking to face of wall and polysulphide sealant between concrete and brickwork","m",1294,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Movement joints","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["3 x 40mm Saw cut joints in top of concrete surface bed ","m",541,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fabric reinforcement","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Type 193 fabric reinforcement in concrete aprons","m2",2389,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["One layer of 250 micron green polyethylene waterproof sheeting sealed at laps with PVC self adhesive tape","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Under aprons","m2",2389,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SPECIALIST FLOOR COVERINGS","H1",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavate in earth or compacted filling not exceeding 2m deep below natural or reduced ground level  ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Reduced levels under pavings, aprons etc","m3",141,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over all excavations for carting away","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over all excavations for carting surplus excavated material and spreading, levelling and lightly compacting on site where directed average 500m from the excavations (Measured nett- no allowance made for bulking)","m3",141,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Compaction of surfaces ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Scarify earth surface to a depth of 150mm, breaking down over size material and reconsolidate to 93% modified AASHTO density ","m2",951,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D12171*C12171","v":{"v":0,"d":"R0.00"}}]
["G5 gravel layers supplied by the contractor compacted to 97% Mod AASHTO density in layers not exceeding 150mm","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Under concrete surfacebed","m3",11,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["G5 gravel layers supplied by the contractor compacted to 93% Mod AASHTO density in layers not exceeding 150mm","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Under artificial grass","m3",130,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["20mm River sand ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Under artificial grass","m2",869,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Mass concrete (30Mpa) in:","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Concrete surfacebed","m3",8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Finishing top surfaces of concrete to an evenly brushed non-slip surface","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Aprons, paving, ramps, etc.","m2",82,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["General Formwork","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Edges, risers, ends and reveals not exceeding 300mm high or wide","m",52,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Movement joints","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["3 x 40mm Saw cut joints in top of concrete surface bed ","m",31,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fabric reinforcement","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Type 193 fabric reinforcement in concrete surface beds, slabs, etc. ","m2",82,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Rubber play surface","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Specialist Play area surface finish: Safety matting called MasterPlay which consists of a composite of a 60mm wearing layer (by MasterFibre® or similar approved) in colours red, blue and orange. Top coat and hardwearing sealer included on full area","m2",82,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Artificial turf","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Artificial turf to be supplied and layed on top of 20mm sand bedding (measured elsewhere), with at least 5/8” tufted filament synthetic grass carpet, with 50% river sand & 50% rubber infill, laid in straight stitch pattern with pile content of 100% polyethylene monofilament U.V -resistant, 13.800/8 dTex, ","m2",869,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SUNDRIES","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Bollards","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Supply and install standard 90x3mm hot dipped galvanized pipe, 1200mm long (300mm below and 900mm above ground), embedded in 490 x 490 x 240mm concrete (20MPa) base including excavations and backfilling. Sample to be provided for approval by Landscape Architect before manufacture","No",200,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Supply and install \"Minister\" type hot dipped galvanised steel (140kg) bollards, 1200mm long (300mm below and 900mm above ground), embedded in 568 x 568 x 240mm concrete (20MPa) base including excavations and backfilling (See detail drawing LAN-2443-601 at the back of these Bills of Quantities) ","No",30,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Supply and install \"Minister\" type hot dipped galvanised steel (140kg) removable bollards including galvanised sleeve to fit bollard and localised cover plate, 1200mm long (300mm below and 900mm above ground), embedded in 568 x 568 x 240mm concrete (20MPa) base including excavations and backfilling (See detail drawing LAN-2443-601 at the back of these Bills of Quantities) ","No",9,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Supply and install \"Half Penny\" type (185kg) concrete bollards with smooth concrete finish, embedded in 450 x 450 x 200mm concrete (20MPa) base including excavations and backfilling (See detail drawing LAN-2443-601 at the back of these Bills of Quantities) ","No",300,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Galvanised Steel Bins","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Supply and install Square hot dipped galvanized perforated/laser cut steel bins, 1000mm high, 450mm diameter as per detail, embedded in 300 x 300 x 300mm concrete (20MPa) base including excavations and backfilling. Sample to be provided for approval by Landscape Architect before manufacture. (See detail drawing LAN-2443-601 at the back of these Bills of Quantities) ","No",60,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Supply and install Round hot dipped galvanized perforated/laser cut steel bins, 1000mm high, 450mm diameter as per detail, embedded in 300 x 300 x 300mm concrete (20MPa) base including excavations and backfilling. Sample to be provided for approval by Landscape Architect before manufacture. (See detail drawing LAN-2443-601 at the back of these Bills of Quantities) ","No",25,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Tree Grids","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Supply and install Square 1200 x 1200 x 25mm galvanised mentis grid tree grate to fit in galvanised frame size 75 x 25 x 5mm thick manufactured in two halves and bolted and track-welded together. Frame to be embedded in 200 x 200mm concrete (20MPa) collar including excavations and backfilling. Sample to be provided for approval by Landscape Architect before manufacture. (See detail drawing LAN-2443-601 at the back of these Bills of Quantities) ","No",24,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Supply and install Round 2000mm dia. x 25mm thick galvanised mentis grid tree grate to fit in galvanised frame size 75 x 25 x 5mm thick manufactured in two halves and bolted and track-welded together. Frame to be embedded in 200 x 200mm concrete (20MPa) collar including excavations and backfilling. Sample to be provided for approval by Landscape Architect before manufacture. (See detail drawing LAN-2443-601 at the back of these Bills of Quantities) ","No",60,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D12235*C12235","v":{"v":0,"d":"R0.00"}}]
["Cycle Racks","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Supply and install 60mm Dia. Galvanized steel 'Ribbon' cycle rack, size 1575 x 1200mm long (300mm below and 900mm above ground), embedded in 460 x 615 x 300mm concrete (15MPa) base on both sides with 1010 x 615 x 100mm surface bed in between bases, with a smooth concrete finish with steel trowel, including excavations and backfilling (See detail drawing LAN-2443-601 at the back of these Bills of Quantities) ","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Concrete stepping Stones","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Supply and install 600 x 600 x 50mm concrete stepping stones, including soil preparation, compaction, sand bedding and finishing off","No",50,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Concrete Benches","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Supply and install 1500 x 450 x 450mm high concrete \"Turin\" bench by Wilson Stone or similar approved with smooth concrete finish, embedded in 500 x 300 x 200mm concrete (15MPa) base including excavations and backfilling (See detail drawing LAN-2443-601 at the back of these Bills of Quantities) ","No",125,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Relocate existing aloes","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Locate 1000mm to 2000mm diameter aloe, clear and lift existing aloes as pointed out on site, replant aloes temporary in secure area and watered every 14 days. Aloe to be replanted to final position as identified by Landscape architect","No",60,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Locate smaller than 1000mm diameter aloe, clear and lift existing aloes as pointed out on site, replant aloes temporary in secure area and watered every 14 days. Aloe to be replanted to final position as identified by Landscape architect","No",60,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Steel Artwork","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Provide the sum of R1,000,000.00 (One Million Rand) nett for Steel Artwork Installation","Item",1,{"v":1000000,"d":"R1,000,000.00"},{"v":1000000,"d":"R1,000,000.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for profit if required ","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for attendance ","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TOTAL LANDSCAPING ",null,0,null,{"$f":"SUM(E11945:E12261)","v":{"v":1000000,"d":"1,000,000.00"}}]
[null,null,0,null,{"v":0,"d":"R0.00"}]
["SECTION 4","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["EXTERNAL WORKS (PROVISIONAL)","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["BILL NO 5","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["STORMWATER DRAINAGE ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PREAMBLES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Preambles for Trades as defined in Scope of Work (C3.1 Item 4.1 & Item 4.2)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TRADE NAMES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Any reference to trade names  in the Bills of Quantities or Architect's specification or drawings shall deem to mean \"or similar and approved\"",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SUPPLEMENTARY PREAMBLES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE :All Civil works to be carried out in accordance with the standardised SABS 1200 specifications",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 146 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["EARTHWORKS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavations in earth","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["For pipes not exceeding 1m deep","m3",2976,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["For pipes exceeding 1m and not exceeding 2m deep","m3",5922,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["For pipes exceeding 2m and not exceeding 3m deep","m3",6743,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["For pipes exceeding 3m and not exceeding 4m deep","m3",1353,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over excavations for carting away ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D12299*C12299","v":{"v":0,"d":"R0.00"}}]
["Surplus material from excavations and/or stock piles on site to a dumping site to be located by the contractor ","m3",8051,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over excavations in earth for excavation in","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Intermediate rock","m3",1699,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Hard rock","m3",1699,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["BEDDING, BACKFILLING, ETC","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Filling from excavations including sifting and compaction to 93% MOD AASHTO density for backfilling to","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Pipe trenches ","m3",8983,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Provide bedding (Blanket) from trench excavations in layers not exceeding 150mm thick, compacted to 93% MOD AASHTO density","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Selected granular material ","m3",324,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Selected fill material ","m3",640,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Carted on selected material from commercial sources including sifting and compaction to 98% MOD AASHTO density for backfilling to","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Selected granular material ","m3",1102,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Selected fill material ","m3",4490,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PIPEWORK","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["oPVC pipes Heavy duty Class 34 for use under ground in accordance with SABS 791 with uPVC couplings  (pipes including excavating in earth, bedding, backfilling and compaction and disposal of surplus material) ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["75mm Diameter pipe not exceeding 1m deep","m",596,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110mm Diameter pipe not exceeding 1m deep","m",770,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["160mm Diameter pipe not exceeding 1m deep","m",747,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["200mm Diameter pipe not exceeding 1m deep","m",283,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over oPVC pipes for fittings","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["75mm Junction","No",12,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["75mm Bend, 45 degrees","No",104,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110 x 75mm Reducer","No",18,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110 x 75mm Reducing junction","No",40,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110mm Junction","No",17,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110mm Bend, 45 degrees","No",137,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["160 x 110mm Reducer","No",14,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["160 x 110mm Reducing juntion","No",42,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["160mm Bend, 45 degrees","No",116,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["200 x 160mm Reducer","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["200 x 160mm Reducing junction","No",27,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["200mm Bend, 45 degrees","No",49,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D12363*C12363","v":{"v":0,"d":"R0.00"}}]
["Supply and lay Class 100D spigot and socket joint reinforced concrete pipes (excavation, backfilling, compaction, etc. elsewhere)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150mm Diameter pipe exceeding 1m and not exceeding 2m deep","m",40,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150mm Diameter pipe exceeding 2m and not exceeding 3m deep","m",76,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["225mm Diameter pipe not exceeding 1m deep","m",51,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["225mm Diameter pipe exceeding 1m and not exceeding 2m deep","m",12,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["375mm Diameter pipe not exceeding 1m deep","m",1127,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["375mm Diameter pipe exceeding 1m and not exceeding 2m deep","m",2491,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["375mm Diameter pipe exceeding 2m and not exceeding 3m deep","m",421,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["375mm Diameter pipe exceeding 3m and not exceeding 4m deep","m",42,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["450mm Diameter pipe not exceeding 1m deep","m",11,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["450mm Diameter pipe exceeding 1m and not exceeding 2m deep","m",179,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["450mm Diameter pipe exceeding 2m and not exceeding 3m deep","m",123,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["450mm Diameter pipe exceeding 3m and not exceeding 4m deep","m",14,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["525mm Diameter pipe exceeding 1m and not exceeding 2m deep","m",167,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["525mm Diameter pipe exceeding 2m and not exceeding 3m deep","m",93,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["525mm Diameter pipe exceeding 3m and not exceeding 4m deep","m",30,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["600mm Diameter pipe exceeding 1m and not exceeding 2m deep","m",55,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["600mm Diameter pipe exceeding 2m and not exceeding 3m deep","m",10,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["600mm Diameter pipe exceeding 3m and not exceeding 4m deep","m",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["675mm Diameter pipe exceeding 2m and not exceeding 3m deep","m",58,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["750mm Diameter pipe not exceeding 1m deep","m",47,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["750mm Diameter pipe exceeding 1m and not exceeding 2m deep","m",93,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["750mm Diameter pipe exceeding 2m and not exceeding 3m deep","m",69,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["825mm Diameter pipe exceeding 2m and not exceeding 3m deep","m",64,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["900mm Diameter pipe exceeding 1m and not exceeding 2m deep","m",43,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["900mm Diameter pipe exceeding 2m and not exceeding 3m deep","m",255,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["1050mm Diameter pipe exceeding 1m and not exceeding 2m deep","m",30,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["1050mm Diameter pipe exceeding 2m and not exceeding 3m deep","m",407,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["1050mm Diameter pipe exceeding 3m and not exceeding 4m deep","m",125,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["1200mm Diameter pipe exceeding 2m and not exceeding 3m deep","m",43,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["MANHOLES, KERB INLETS, CHAMBERS, ETC","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavate in earth for and build composite manhole formed  of one brick walls minimum 600mm high, from engineering bricks, finished externally with one coat cement plaster and a bagged finish internally,  on 150mm thick 25Mpa/19mm mass concrete slab with 20Mpa fine mass concrete benching in bottom, floated smooth with falls including all necessary  bends, junctions etc. Install 1000mm internal diameter precast concrete rings, for remainder of depth of manhole complete, including all necessary excavations, precast manholes rings, 150mm reinforced concrete cover slab with opening for cast iron cover and frame (measured  elsewhere) including step irons at 300mm centres vertically and staggered 300mm in cement mortar and sealed in tallow","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D12427*C12427","v":{"v":0,"d":"R0.00"}}]
["Manhole not exceeding 1m deep","No",9,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Manhole exceeding 1m and not exceeding 2m deep","No",49,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Manhole exceeding 2m and not exceeding 3m deep","No",10,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavate in earth for and build composite manhole formed  of one brick walls minimum 600mm high, from engineering bricks, finished externally with one coat cement plaster and a bagged finish internally,  on 150mm thick 25Mpa/19mm mass concrete slab with 20Mpa fine mass concrete benching in bottom, floated smooth with falls including all necessary  bends, junctions etc. Install 1250mm internal diameter precast concrete rings, for remainder of depth of manhole complete, including all necessary excavations, precast manholes rings, 150mm reinforced concrete cover slab with opening for cast iron cover and frame (measured  elsewhere) including step irons at 300mm centres vertically and staggered 300mm in cement mortar and sealed in tallow","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Manhole exceeding 1m and not exceeding 2m deep","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Manhole exceeding 2m and not exceeding 3m deep","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavate in earth for and build composite manhole formed  of one brick walls minimum 975mm high, from engineering bricks, finished externally with one coat cement plaster and a bagged finish internally,  on 150mm thick 25Mpa/19mm mass concrete slab with 20Mpa fine mass concrete benching in bottom, floated smooth with falls including all necessary  bends, junctions etc. Install 1000mm internal diameter precast concrete rings, for remainder of depth of manhole complete, including all necessary excavations, precast manholes rings, 150mm reinforced concrete cover slab with opening for cast iron cover and frame (measured  elsewhere) including step irons at 300mm centres vertically and staggered 300mm in cement mortar and sealed in tallow","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Manhole exceeding 1m and not exceeding 2m deep","No",9,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Manhole exceeding 2m and not exceeding 3m deep","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Manhole exceeding 3m and not exceeding 4m deep","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavate in earth for and build composite manhole formed  of one brick walls minimum 975mm high, from engineering bricks, finished externally with one coat cement plaster and a bagged finish internally,  on 150mm thick 25Mpa/19mm mass concrete slab with 20Mpa fine mass concrete benching in bottom, floated smooth with falls including all necessary  bends, junctions etc. Install 1250mm internal diameter precast concrete rings, for remainder of depth of manhole complete, including all necessary excavations, precast manholes rings, 150mm reinforced concrete cover slab with opening for cast iron cover and frame (measured  elsewhere) including step irons at 300mm centres vertically and staggered 300mm in cement mortar and sealed in tallow","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Manhole exceeding 1m and not exceeding 2m deep","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Manhole exceeding 2m and not exceeding 3m deep","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavate in earth for and build composite manhole formed  of one brick walls minimum 975mm high, from engineering bricks, finished externally with one coat cement plaster and a bagged finish internally,  on 150mm thick 25Mpa/19mm mass concrete slab with 20Mpa fine mass concrete benching in bottom, floated smooth with falls including all necessary  bends, junctions etc. Install 1500mm internal diameter precast concrete rings, for remainder of depth of manhole complete, including all necessary excavations, precast manholes rings, 150mm reinforced concrete cover slab with opening for cast iron cover and frame (measured  elsewhere) including step irons at 300mm centres vertically and staggered 300mm in cement mortar and sealed in tallow","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Manhole exceeding 1m and not exceeding 2m deep","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Manhole exceeding 2m and not exceeding 3m deep","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavate in earth for and build composite manhole formed  of one brick walls minimum 1350mm high, from engineering bricks, finished externally with one coat cement plaster and a bagged finish internally,  on 150mm thick 25Mpa/19mm mass concrete slab with 20Mpa fine mass concrete benching in bottom, floated smooth with falls including all necessary  bends, junctions etc. Install 1000mm internal diameter precast concrete rings, for remainder of depth of manhole complete, including all necessary excavations, precast manholes rings, 150mm reinforced concrete cover slab with opening for cast iron cover and frame (measured  elsewhere) including step irons at 300mm centres vertically and staggered 300mm in cement mortar and sealed in tallow","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Manhole exceeding 2m and not exceeding 3m deep","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavate in earth for and build composite manhole formed  of one brick walls minimum 1350mm high, from engineering bricks, finished externally with one coat cement plaster and a bagged finish internally,  on 150mm thick 25Mpa/19mm mass concrete slab with 20Mpa fine mass concrete benching in bottom, floated smooth with falls including all necessary  bends, junctions etc. Install 1250mm internal diameter precast concrete rings, for remainder of depth of manhole complete, including all necessary excavations, precast manholes rings, 150mm reinforced concrete cover slab with opening for cast iron cover and frame (measured  elsewhere) including step irons at 300mm centres vertically and staggered 300mm in cement mortar and sealed in tallow","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Manhole exceeding 1m and not exceeding 2m deep","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Manhole exceeding 2m and not exceeding 3m deep","No",19,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Manhole exceeding 3m and not exceeding 4m deep","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavate in earth for and build composite manhole formed  of one brick walls minimum 1350mm high, from engineering bricks, finished externally with one coat cement plaster and a bagged finish internally,  on 150mm thick 25Mpa/19mm mass concrete slab with 20Mpa fine mass concrete benching in bottom, floated smooth with falls including all necessary  bends, junctions etc. Install 1500mm internal diameter precast concrete rings, for remainder of depth of manhole complete, including all necessary excavations, precast manholes rings, 150mm reinforced concrete cover slab with opening for cast iron cover and frame (measured  elsewhere) including step irons at 300mm centres vertically and staggered 300mm in cement mortar and sealed in tallow","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Manhole exceeding 2m and not exceeding 3m deep","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Manhole exceeding 3m and not exceeding 4m deep","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavate in earth for and build composite manhole formed  of one brick walls minimum 1350mm high, from engineering bricks, finished externally with one coat cement plaster and a bagged finish internally,  on 150mm thick 25Mpa/19mm mass concrete slab with 20Mpa fine mass concrete benching in bottom, floated smooth with falls including all necessary  bends, junctions etc. Install 1800mm internal diameter precast concrete rings, for remainder of depth of manhole complete, including all necessary excavations, precast manholes rings, 150mm reinforced concrete cover slab with opening for cast iron cover and frame (measured  elsewhere) including step irons at 300mm centres vertically and staggered 300mm in cement mortar and sealed in tallow","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Manhole exceeding 2m and not exceeding 3m deep","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavate in earth for and build stormwater double grid catchpit, size 1762 x 1000mm not exceeding 1m deep internally, with one brick sides, finished internally with one coat cement plaster, on 150mm thick reinforced concrete 25Mpa (20mm stone) base to project 75mm all round and reinforced with and including 20mm diameter high tensile reinforcing bars at 200mm centres in both directions, with 100mm thick precast concrete cover slab,  finished smooth on all exposed surfaces, rounded on salient angles and provided with opening rebated for grating (measured elsewhere), including concrete benching, building through pipes, formwork, back filling, ramming, etc. ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Double grid catchpit not exceeding 1m deep","No",19,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Double grid catchpit exceeding 1m and not exceeding 2m deep","No",14,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Double grid catchpit exceeding 2m and not exceeding 3m deep","No",13,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavate in earth for and build stormwater single grid catchpit, size 880 x 850mm not exceeding 1m deep internally, with one brick sides, finished internally with one coat cement plaster, on 150mm thick reinforced concrete 25Mpa (20mm stone) base to project 75mm all round and reinforced with and including 20mm diameter high tensile reinforcing bars at 200mm centres in both directions, with 100mm thick precast concrete cover slab,  finished smooth on all exposed surfaces, rounded on salient angles and provided with opening rebated for grating (measured elsewhere), including concrete benching, building through pipes, formwork, back filling, ramming, etc. ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D12491*C12491","v":{"v":0,"d":"R0.00"}}]
["Single grid catchpit not exceeding 1m deep","No",50,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Single grid catchpit exceeding 1m and not exceeding 2m deep","No",16,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Single grid catchpit exceeding 2m and not exceeding 3m deep","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Kerb inlet extreme size 2260 x 1807mm on 150mm 25MPa concrete base, one brick walls plastered externally and bag finished internally, 150mm 30MPa reinforced concrete cover slab 2260 x 1100mm reinforced with ref 617 mesh with opening for type 2B cover and frame (measured elsewhere), two fig 4 precast lintel kerbs (1000mm in length) and 330 x 330m  brick pier in separating inlet section. Inlet to receive two 450 x 600mm cast iron frames (measured elsewhere). All on 150mm 30Mpa concrete bottom slab protruding 50mm all round with 25MPa concrete sloping to discharge pipe","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Kerb inlet exceeding 1m deep","No",10,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Kerb inlet exceeding 1m and not exceeding 2m deep","No",45,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over stromwater structures for additional pipe openings","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Form opening through wall for 75mm pipe","No",9,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Form opening through wall for 110mm pipe","No",29,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Form opening through wall for 160mm pipe","No",47,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Form opening through wall for 200mm pipe","No",63,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Gratings, covers, etc","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["550mm Diameter Type 2A cast iron manhole cover and frame, with frame bedded in 3:1 cement mortar and cover sealed in tallow. ","No",131,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["450 x 600mm Double hinged cast iron grating and frame bedded in cement mortar","No",270,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Type 2B DI snap lock cover and frame class D400 cast into concrete slab","No",55,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["1500 x 1500mm hinged fitted steel mentis grating sand trap with clip lock at the bottom, internally fixed to stormwater structure ","No",11,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["1200 x 1200mm hinged fitted steel mentis grating sand trap with clip lock at the bottom, internally fixed to stormwater structure ","No",14,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["1050 x 1050mm hinged fitted steel mentis grating sand trap with clip lock at the bottom, internally fixed to stormwater structure ","No",9,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["975 x 975mm hinged fitted steel mentis grating sand trap with clip lock at the bottom, internally fixed to stormwater structure ","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["900 x 900mm hinged fitted steel mentis grating sand trap with clip lock at the bottom, internally fixed to stormwater structure ","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["750 x 750mm hinged fitted steel mentis grating sand trap with clip lock at the bottom, internally fixed to stormwater structure ","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["675 x 675mm hinged fitted steel mentis grating sand trap with clip lock at the bottom, internally fixed to stormwater structure ","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["600 x 600mm hinged fitted steel mentis grating sand trap with clip lock at the bottom, internally fixed to stormwater structure ","No",18,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["525 x 525mm hinged fitted steel mentis grating sand trap with clip lock at the bottom, internally fixed to stormwater structure ","No",27,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["375 x 375mm hinged fitted steel mentis grating sand trap with clip lock at the bottom, internally fixed to stormwater structure ","No",7,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["300 x 300mm hinged fitted steel mentis grating sand trap with clip lock at the bottom, internally fixed to stormwater structure ","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["STORMWATER GULLEY INLETS","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavate in earth for and build stormwater single grid catchpit, size 265 x 265mm not exceeding 1m deep internally, with one brick sides, finished internally with one coat cement plaster, on 150mm thick reinforced concrete 25Mpa (20mm stone) base to project 75mm all round and reinforced with and including 20mm diameter high tensile reinforcing bars at 200mm centres in both directions, with 100mm thick precast concrete cover slab,  finished smooth on all exposed surfaces, rounded on salient angles and provided with opening rebated for grating (measured elsewhere), including concrete benching, building through pipes, formwork, back filling, ramming, etc. ","No",50,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Gratings, covers, etc","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["265 X 265mm cast iron light duty dished grating and fame, type SABS 1115 Fig. 3","No",50,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["STORMWATER GRID CHANNEL","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavate in earth for and build stormwater channel formed  of one brick walls minimum 600mm high, plastered on the inside with cement plaster (5:1),  on 150mm  thick 25Mpa/19mm  reinforced concrete slab including Y12 bars at 200c/c in both directions with 20Mpa fine mass  concrete  benching in bottom, floated smooth with falls including all necessary  bends, junctions  etc., including all necessary excavations, 150mm reinforced concrete roof slab including Y12 bars at 200 c/c in both directions with opening for grid channel 450mm wide (measured  elsewhere) ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D12555*C12555","v":{"v":0,"d":"R0.00"}}]
["Grid stormwater channel","m",14,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Angle sections","t",0.1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["RSA40 (40 x 5.5) Rectagrid channel cover","m2",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The following in grass stormwater channels","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavate to form stormwater channel with 45 degree sloping sides 1m wide at bottom of channel and not exceeding 1000mm deep, with 150mm layer from excavations compacted to 93% Mod AASHTO density and 150mm layer of topsoil to receive natural occurring grass","m",396,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Natural occurring grass to stromwater channel","m2",1774,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TESTS, ETC.","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Provide all necessary apparatus, etc for and test the whole of the Stormwater Drainage system to the satisfaction of the Representative/Agent, rectify all defective work free of charge and leave in perfect order","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SUBSOIL DRAINAGE","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavations in earth","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["For pipes not exceeding 1m deep","m3",2209,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["For pipes exceeding 1m and not exceeding 2m deep","m3",74,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over excavations in earth for excavation in","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Soft rock","m3",228,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Hard rock","m3",228,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over all excavations for carting away","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Surplus material from excavations and/or stock piles on site to a dumping site to be located by the contractor","m3",1141,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Approved G7 filling supplied and carted on by the Contractor, compacted in layers not exceeding 150mm to 93% Mod. AASHTO density","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Backfilling to trenches, bases, etc. ","m3",1141,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Approved 19mm Stone layer under lower ground parking area","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["300 X 300mm 19mm stone in backfilling to trench around pipe","m3",338,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Approved free draining compactable material such as well graded clean washed sand or gravel supplied and carted on by the Contractor, compacted in layers not exceeding 150mm to 95% Mod. AASHTO density","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Backfilling to trenches not exceeding 300mm wide","m3",804,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["GEOTEXTILE","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["A2 bidum geotextile material","m2",4500,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Subsoil drain","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Subsoil drain formed with 110mm UPVC perforated geopipe, wrapped in A2 bidum geotextile material","m",3287,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Subsoil drain formed with 160mm UPVC perforated geopipe, wrapped in A2 bidum geotextile material","m",319,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Subsoil drain formed with 200mm UPVC perforated geopipe, wrapped in A2 bidum geotextile material","m",144,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over uPVC perforated pipes for fittings","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110mm Bend, 11.25 degrees","No",8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110mm Bend, 22.5 degrees","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D12619*C12619","v":{"v":0,"d":"R0.00"}}]
["110mm Bend, 45 degrees","No",229,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110mm Y-juntion","No",40,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["160mm Bend, 45 degrees","No",11,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["160 x 100mm Reducing Y-juntion","No",95,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["200mm Bend, 22.5 degrees","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["200mm Bend, 45 degrees","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["200mm Y-juntion","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["200 x 110mm Reducing Y-juntion","No",32,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["200 x 160mm Reducing Y-juntion","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SUBSOIL DRAINS BEHIND RETAINING AND BUND WALLS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Approved free draining compactable material such as well graded clean washed sand or gravel supplied and carted on by the Contractor, compacted in layers not exceeding 150mm to 95% Mod. AASHTO density","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Backfilling to trenches not exceeding 300mm wide","m3",401,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Subsoil drain formed with 110mm UPVC perforated geopipe, wrapped in A2 bidum geotextile material","m",1338,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["HEADWALLS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The following in No. 4 headwalls","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavate in earth not exceeding 2.0m deep below reduced or natural ground level ","m3",40,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for risk of collapse to sides of excavations not exceeding 1.5m deep","m2",108,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Backfilling with excavated material in trenches, etc. against walls, etc.","m3",16,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over all excavations for loading and carting away surplus material from site","m3",24,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["25 MPa/19 mm concrete in base ","m3",8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["One brick wall in stretcher bond in 4:1 cement mortar","m2",64,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["One coat 4:1 cement plaster on brick walls","m2",64,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["One coat 4:1 cement plaster in narrow widths","m2",12,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Bell mouthed stormwater outlet, internal size 1800mm wide at inlet, bell mouthed to 3300mm at outlet and 3000mm long, formed with minimum 150mm thick concrete 20MPa  (20mm stone) base on Mesh 245, provided with fourteen bricks, laid on and including \"USB Green\" dampproofing, cast 50mm deep into top surface of base, all concrete finished smooth on all exposed surfaces, including necessary excavation, back filling, ramming and smooth formwork ","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["One layer stone pitching to stormwater outlets, formed  with approved stone with diameter varying from 150mm to 200mm, laid loose and randomly close to each other on ground, including all necessary shallow excavation, filling, ramming, etc","m2",28,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["STORMWATER DETENTION POND FOREBAYS AND OUTLET STRUCTURE","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["EARTHWORKS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavation in earth or compacted filling not exceeding 2m deep","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Reducing levels to final levels under floors, ramps, pavings, etc. ","m3",497,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Trenches","m3",347,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sumps","m3",11,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavation in earth or compacted filling  exceeding 2m not exceeding 4m deep","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D12683*C12683","v":{"v":0,"d":"R0.00"}}]
["Reducing levels to final levels under floors, ramps, pavings, etc. ","m3",186,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Trenches","m3",193,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Holes","m3",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavation in earth or compacted filling  exceeding 4m not exceeding 6m deep","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Trenches","m3",7,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over excavations in earth for excavation in","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Soft rock","m3",115,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Hard rock","m3",57,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over all excavations for carting away","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Surplus material from excavations and/or stock piles on site to a dumping site to be located by the contractor","m3",988,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Risk of collapse of excavations","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sides of trench and hole excavations not exceeding 1,5m deep","m2",16,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but exceeding 3m deep and not exceeding 4.5m deep","m2",459,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Back excavation of vertical sides of excavation in earth, for working space, including backfilling compacted to 93% Mod AASHTO density","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Exceeding 1,5m and not exceeding 3m deep approximately 1,5m away from face of building including backfilling and compaction to 93% mod AASHTO density ","m2",378,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Exceeding 3m and not exceeding 4,5m deep approximately 1,5m away from face of building including backfilling and compaction to 93% mod AASHTO density ","m2",17,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Exceeding 4,5m and not exceeding 6m deep approximately 1,5m away from face of building including backfilling and compaction to 93% mod AASHTO density ","m2",30,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Selected earth filling obtained from the excavations and/or prescribed stock piles on site in layers of 150mm thick compacted to 93% Mod AASHTO density","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Backfilling to trenches, holes, etc","m3",215,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Selected earth filling obtained from the excavations and/or prescribed stock piles on site in layers of 150mm thick compacted to 95% Mod AASHTO density","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Under floors, steps, pavings, etc","m3",40,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Compaction of surfaces ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Compaction of ground surface under surface beds etc including scarifying for a depth of 150mm, breaking down oversize material, adding suitable material where necessary and compacting to 93% Mod AASHTO density","m2",389,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Detention pond surfaces ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Scarifying for a depth of 150mm, breaking down oversize material, adding suitable material where necessary and no compacting","m2",1564,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Tiffsport type grass or similar approved closely packed and top dressed as necessary to even surfaces","m2",1564,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["UNREINFORCED CONCRETE CAST AGAINST EXCAVATED SURFACES ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["30MPa Mass concrete","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Aprons","m3",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["REINFORCED CONCRETE CAST AGAINST EXCAVATED SURFACES ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["25MPa/19mm concrete","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Strip footings","m3",53,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D12747*C12747","v":{"v":0,"d":"R0.00"}}]
["Surface beds","m3",38,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["30 MPa/19 mm concrete in","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Surface beds","m3",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["REINFORCED CONCRETE ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["25 MPa/19 mm concrete in","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Walls","m3",80,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sump walls","m3",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["30 MPa/19 mm concrete in","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Walls","m3",7,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["ROUGH FORMWORK (DEGREE OF ACCURACY II)","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Rough formwork to sides","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Walls exceeding 3.5m and not exceeding 5m high","m2",847,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Walls exceeding 5m and not exceeding 6.5m high","m2",45,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Boxing in rough formwork to form:","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Opening size 2000 x 500mm high in 200mm thick concrete wall","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["REINFORCEMENT","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Mild tensile steel rod reinforcement to structural concrete ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["8mm Diameter bars","t",1.45,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["High tensile steel rod reinforcement to structural concrete ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["10mm Diameter bars","t",1.45,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["12mm Diameter bars","t",4.35,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["16mm Diameter bars","t",4.35,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["20mm Diameter bars","t",2.9,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fabric reinforcement","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Type 395 fabric reinforcement in concrete surface bed, slabs, etc.","m2",378,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Armorflex block overflow ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavation in earth or compacted filling not exceeding 2m deep","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Reducing levels to final levels under floors, ramps, pavings, etc. ","m3",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over all excavations for carting away","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Surplus material from excavations and/or stock piles on site to a dumping site to be located by the contractor","m3",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Compaction of surfaces ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Compaction of ground surface under surface beds etc including scarifying for a depth of 150mm, breaking down oversize material, adding suitable material where necessary and compacting to 93% Mod AASHTO density","m2",22,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D12811*C12811","v":{"v":0,"d":"R0.00"}}]
["Approved G5 filling supplied and carted on by the Contractor, compacted in layers not exceeding 150mm to 95% Mod. AASHTO density","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Under solid floors ","m3",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["20mm Thick coarse river sand filling supplied by the contractor","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Under floors etc","m2",22,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Armorflex blocks","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Concor Armorflex 140 or equal approved as by Concor Technicrete 25MPa blocks size 340 x 400 x 95mm high in overland weir, installed strictly according to manufacturer's specification","m2",22,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["A2 bidum geotextile material","m2",22,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TOTAL STORMWATER DRAINAGE ",null,0,null,{"$f":"SUM(E12263:E12825)","v":{"v":0,"d":"0.00"}}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SECTION 4","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["EXTERNAL WORKS (PROVISIONAL)","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["BILL NO 6","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SOIL DRAINAGE ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PREAMBLES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Preambles for Trades as defined in Scope of Work (C3.1 Item 4.1 & Item 4.2)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TRADE NAMES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Any reference to trade names  in the Bills of Quantities or Architect's specification or drawings shall deem to mean \"or similar and approved\"",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SUPPLEMENTARY PREAMBLES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE :All Civil works to be carried out in accordance with the standardised SABS 1200 specifications",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 146 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["EARTHWORKS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavations in earth","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["For pipes not exceeding 1m deep","m3",1703,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["For pipes exceeding 1m and not exceeding 2m deep","m3",3155,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["For pipes exceeding 2m and not exceeding 3m deep","m3",1641,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["For pipes exceeding 4m and not exceeding 5m deep","m3",581,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over excavations for carting away ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Surplus material from excavations and/or stock piles on site to a dumping site to be located by the contractor ","m3",2516,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["BEDDING, BACKFILLING, ETC","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Filling from excavations including sifting and compaction to 93% MOD AASHTO density for backfilling to","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Pipe trenches ","m3",4606,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Carted on selected material from commercial sources including sifting and compaction to 98% MOD AASHTO density for backfilling to","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Selected granular material ","m3",556,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D12875*C12875","v":{"v":0,"d":"R0.00"}}]
["Selected fill material ","m3",1838,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PIPEWORK","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["uPVC pipes Heavy duty Class 34 for use under ground in accordance with SABS 791 with uPVC couplings (Excavation, bedding material, back filling, compaction, etc. elsewhere)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["160mm Diameter pipe not exceeding 1m deep","m",1969,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["160mm Diameter pipe exceeding 1m and not exceeding 2m deep","m",1781,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["160mm Diameter pipe exceeding 2m and not exceeding 3m deep","m",145,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["200mm Diameter pipe not exceeding 1m deep","m",258,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["200mm Diameter pipe exceeding 1m and not exceeding 2m deep","m",441,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["200mm Diameter pipe exceeding 2m and not exceeding 3m deep","m",583,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["200mm Diameter pipe exceeding 3m and not exceeding 4m deep","m",125,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["200mm Diameter pipe exceeding 4m and not exceeding 5m deep","m",51,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over uPVC pipes for fittings","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["160mm Bend, 11.25 degrees","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["160mm Bend, 22.5 degrees","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["160mm Bend, 45 degrees","No",9,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["160mm Y-Junction","No",15,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sundries","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over excavation in earth for pipe trenches, chambers, etc for excavation in intermediate rock","m3",708,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over excavation in earth for pipe trenches, chambers, etc for excavation in hard rock","m3",708,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Mass concrete Class C encasing to horizontal pipes","m3",158,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Mass concrete Class C encasing to vertical pipes","m3",95,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["MANHOLES, ETC","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Factory cast fibre cement manholes including base, 1000mm internal diameter, complete including all necessary excavations, in situ concrete bottom slabs haunched around fibre cement base (size 1600mm diameter) (min thickness of slab 150mm and maximum thickness 350mm), 170mm thick medium duty precast cover slab with 560mm diameter opening, channels, finishes, polypropelene or calcamite steps staggered at 300mm centres, cast iron double seal manhole cover and frame (cover and frame elsewhere measured), etc. all joints sealed with \"SIKAFLEX-PRO 2HP\" or similar approved","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Manhole not exceeding 1m deep","No",45,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Manhole exceeding 1m and not exceeding 2m deep","No",55,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Manhole exceeding 2m and not exceeding 3m deep","No",36,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Manhole exceeding 3m and not exceeding 4m deep","No",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Manhole exceeding 4m and not exceeding 5m deep","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Pipes, fittings and fixtures to backdrop maholes","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["uPVC pipes Heavy duty Class 34 in accordance with SABS 791 with uPVC, fixed to manhole wall with weld attached threaded rod welded to 160mm diameter stainless steel hoop around pipe at maximum 1000mm centres","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["160mm Diameter pipe fixed to manhole wall","m",47,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over uPVC pipes for fittings","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D12939*C12939","v":{"v":0,"d":"R0.00"}}]
["160mm Access junction","No",29,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["160mm Bend, 45 degrees","No",58,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sundries","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["350 x 350 x 305mm high 15Mpa concrete cast around 160mm diameter pipe in penetration seal, including all necessary excavations, formwork, backfilling ect, ","No",29,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Gratings, covers, etc","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["560mm Diameter heavy duty hinged ductile iron manhole cover and frame to EN124 D400, with frame bedded in 3:1 cement mortar and cover sealed in tallow","No",140,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["OFF SITE SOIL DRAINAGE ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["EARTHWORKS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavations in earth","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["For pipes not exceeding 1m deep","m3",39,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["For pipes exceeding 1m and not exceeding 2m deep","m3",1042,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["For pipes exceeding 2m and not exceeding 3m deep","m3",51,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["For pipes exceeding 3m and not exceeding 4m deep","m3",69,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over excavations for carting away ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Surplus material from excavations and/or stock piles on site to a dumping site to be located by the contractor","m3",389,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["BEDDING, BACKFILLING, ETC","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Filling from excavations including sifting and compaction to 93% MOD AASHTO density for backfilling to","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Pipe trenches ","m3",457,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cement stabilized (4% cement) filling from excavations including sifting and compaction to 93% MOD AASHTO density for backfilling to","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Pipe trenches ","m3",362,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Carted on selected material from commercial sources including sifting and compaction to 98% MOD AASHTO density for backfilling to","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Selected granular material ","m3",86,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Selected fill material ","m3",284,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PIPEWORK","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["uPVC pipes Heavy duty Class 34 for use under ground in accordance with SABS 791 with uPVC couplings (Excavation, bedding material, back filling, compaction, etc. elsewhere)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["200mm Diameter pipe not exceeding 1m deep","m",39,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["200mm Diameter pipe exceeding 1m and not exceeding 2m deep","m",564,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["200mm Diameter pipe exceeding 2m and not exceeding 3m deep","m",18,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["200mm Diameter pipe exceeding 3m and not exceeding 4m deep","m",18,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sundries","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over excavation in earth for pipe trenches, chambers, etc for excavation in intermediate rock","m3",120,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over excavation in earth for pipe trenches, chambers, etc for excavation in hard rock","m3",60,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D13003*C13003","v":{"v":0,"d":"R0.00"}}]
["Mass concrete Class C encasing to horizontal pipes","m3",26,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Mass concrete Class C encasing to vertical pipes","m3",15,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Connect to existing sewer line","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Cut into existing precast concrete manhole exceeding 3m and not exceeding 4m deep internally, including all necessary channels, benching, sealing and making good of existing finishes, etc. ","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["MANHOLES, ETC","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavate in earth for and build composite manhole formed  of 4 bricks on edge equally spaced on surround, on 1800mm diameter 100mm thick 20Mpa concrete slab reinforced with ref 617 mesh with 20Mpa/13mm stone mass concrete benching in bottom, floated smooth with falls including all necessary  bends, junctions etc. on a 50mm thick concrete blinding. Install 1000mm internal diameter precast concrete rings, for remainder of depth of manhole complete, including all necessary excavations, precast manholes rings, 150mm reinforced concrete cover slab with opening for cast iron cover and frame (measured  elsewhere), etc. all joints sealed with 1:3 cement sand mix caulked in ring joints","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Manhole not exceeding 1m deep","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Manhole exceeding 1m and not exceeding 2m deep","No",12,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Gratings, covers, etc","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SABS Type 4 medium duty cast iron double seal manhole cover and frame, with frame bedded in 3:1 cement mortar and cover sealed in tallow","No",13,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Testing","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Pressure testing drainage pipe system","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Testing drainage system for open flow by means of drawing a badger through system","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TOTAL SOIL DRAINAGE ",null,0,null,{"$f":"SUM(E12827:E13029)","v":{"v":0,"d":"0.00"}}]
[null,null,0,null,{"v":0,"d":"R0.00"}]
["SECTION 4","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["EXTERNAL WORKS (PROVISIONAL)","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["BILL NO 7","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["EXTERNAL WATER SUPPLY ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PREAMBLES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Preambles for Trades as defined in Scope of Work (C3.1 Item 4.1 & Item 4.2)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TRADE NAMES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Any reference to trade names  in the Bills of Quantities or Architect's specification or drawings shall deem to mean \"or similar and approved\"",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SUPPLEMENTARY PREAMBLES","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE :All Civil works to be carried out in accordance with the standardised SABS 1200 specifications",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NOTE: The following items shall be deemed to fall into Work Group No 146 for JBCC CPAP purposes",{"$nulls":3},{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["WATER SUPPLIES","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["EARTHWORKS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["For pipes not exceeding 1m deep","m3",2317,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over excavations for carting away ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Surplus material from excavations and/or stock piles on site to a dumping site to be located by the contractor","m3",1298,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["BEDDING, BACKFILLING, ETC","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Filling from excavations including sifting and compaction to 93% MOD AASHTO density for backfilling to","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D13067*C13067","v":{"v":0,"d":"R0.00"}}]
["Pipe trenches ","m3",1020,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Carted on G7 sand selected material from commercial sources including sifting and compaction to 98% MOD AASHTO density for backfilling to","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Selected granular material ","m3",250,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Selected fill material ","m3",776,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PIPEWORK","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sterilizing all water pipes prior to installation in strict accordance to the methods and specifications in SANS10252-1","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["HDPE PE100 (PN12.5) pipes in trenches for use under ground in accordance with SABS 791 with compression (Excavation, bedding material, back filling, compaction, etc. elsewhere)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["40mm Diameter pipe not exceeding 1m deep","m",230,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra on HDPE pipes for:","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["40mm HDPE bend","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["uPVC pipes Class 12 for use under ground in accordance with SABS 791 with uPVC couplings (Excavation, bedding material, back filling, compaction, etc. elsewhere)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110mm Diameter pipe not exceeding 1m deep","m",185,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["160mm Diameter pipe not exceeding 1m deep","m",1986,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra on uPVC pipes for flanged bitumen coated hot dipped galvanized steel fittings:","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100mm Bend, 22.5 degrees","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100mm Bend, 45 degrees","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150mm Bend, 11.25 degrees","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150mm Bend, 22.5 degrees","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150mm Bend, 45 degrees","No",13,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150mm Bend, 90 degrees","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150 x 100mm Reducing tee","No",12,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150 x 80mm Reducing tee","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["80 x 40mm Reducer","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["40mm Flange adaptor","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["80mm Flange adaptor","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100mm Flange adaptor","No",18,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150mm Flange adaptor","No",82,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Thrust blocks to 11.25 degree bends","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Size extreme 400 x 350 x 300mm high","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Thrust blocks to 22.5 degree bends","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Size extreme 550 x 400 x 450mm high","No",5,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Thrust blocks to 45 degree bends","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D13131*C13131","v":{"v":0,"d":"R0.00"}}]
["Size extreme 750 x 375 x 600mm high","No",15,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Thrust blocks to 90 degree bends","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Size extreme 1210 x 1210 x 700mm high","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Thrust blocks to T-pieces","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Size extreme 1000 x 500 x 600mm high","No",13,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Taps, Valves, etc.","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100mm Isolating valve ","No",9,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sundries","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over excavation in earth for pipe trenches, chambers, etc for excavation in intermediate rock","m3",232,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over excavation in earth for pipe trenches, chambers, etc for excavation in hard rock","m3",232,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Valve box 750mm internal diameter on 19mm stone base 75mm thick, 100mm pre-cast concrete cover slab including cover and frame 150 x 150 x 100mm cast into frame. (See Drawing 20.00GZA05.D001 attached to the back of these bills of quantities)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Valve Box not exceeding 1m deep","No",9,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Valve Box exceeding 1m and not exceeding 2m deep","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["WATER SUPPLIES TO FIRE APPLIANCES","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["EARTHWORKS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavations in earth","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["For pipes not exceeding 1m deep ","m3",83,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over excavations for carting away","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Surplus material from excavations and/or stock piles on site to a dumping site to be located by the contractor ","m3",47,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["BEDDING, BACKFILLING, ETC","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Filling from excavations including sifting and compaction to 93% MOD AASHTO density for backfilling to","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Pipe trenches ","m3",37,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Carted on material from commercial sources including sifting and compaction to 90% MOD AASHTO density for backfilling to","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Selected granular material ","m3",11,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Selected fill material","m3",35,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PIPEWORK","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["uPVC pipes Class 16 for use under ground in accordance with SABS 791 with uPVC couplings (Excavation, bedding material, back filling, compaction, etc. elsewhere)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110mm Diameter pipe not exceeding 1m deep","m",117,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["160mm Diameter pipe not exceeding 1m deep","m",1150,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Galvanised mild steel pipes to walls","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra on uPVC pipes for flanged bitumen coated hot dipped galvanized steel fittings:","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150mm Bend, 11.25 degrees","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D13195*C13195","v":{"v":0,"d":"R0.00"}}]
["150mm Bend, 22.5 degrees","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150mm Bend, 45 degrees","No",9,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150mm Bend, 90 degrees","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150 x 100mm Reducing tee","No",15,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100mm Flange adaptor","No",15,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150mm Flange adaptor","No",58,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Thrust blocks to 11.25 degree bends","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Size extreme 400 x 350 x 300mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Thrust blocks to 22.5 degree bends","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Size extreme 550 x 400 x 450mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Thrust blocks to 45 degree bends","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Size extreme 750 x 375 x 600mm high","No",11,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Thrust blocks to 90 degree bends","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Size extreme 1210 x 1210 x 700mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Thrust blocks to T-pieces","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Size extreme 1000 x 500 x 600mm high","No",15,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["WATER METERS ETC.","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100mm Combination water meter","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["FIRE HYDRANTS ETC.","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The following in No. 12 fire hydrant assembly","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Concrete Class F shaped pedestal size extreme 350 x 350 x 1200mm high overall finished smooth on exposed surfaces and set 300mm deep in ground including formwork, excavation, etc. including paint to pedestal Golden Yellow BSS 356","No",15,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Hot dipped galvanised screwed steel pipes and fittings as described","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["80mm Diameter pipe 1500mm long","No",15,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["80mm Diameter long radius bend female threaded","No",15,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["80mm Diameter Right angle type tamper proof shielded spindle hydrant valve with 65mm threaded inlet","No",15,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150 x 80mm Reducer","No",15,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["80mm Isolating valve ","No",15,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Hydrant tee on water main","No",15,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["300 x 300 x 100mm Thrust block including all necessary excavations, formwork, etc. ","No",15,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["80 x 300 x 150mm Concrete block including all necessary excavations, formwork, etc. ","No",15,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["BOOSTER CONNECTION.","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The following in No. 2 booster connection assembly","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D13259*C13259","v":{"v":0,"d":"R0.00"}}]
["Concrete Class F shaped pedestal size extreme 305 x 305 x 915mm high overall finished smooth on exposed surfaces and set 305mm deep in ground including formwork, excavation, etc. including paint to pedestal Yellow","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Hot dipped galvanised screwed steel pipes and fittings as described","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100mm Diameter pipe 1500mm long","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100mm Diameter long radius bend female threaded","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["65mm Diameter female bayonet couplings with end caps and chain","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100 x 50mm Reducer","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150mm x 2400kPa pressure meter ","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100mm Equal tee","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sundries","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over excavation in earth for pipe trenches, chambers, etc for excavation in intermediate rock","m3",8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over excavation in earth for pipe trenches, chambers, etc for excavation in hard rock","m3",8,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["WATER RETICULATION TO IRRIGATION SYSTEM","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["EARTHWORKS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["For pipes not exceeding 1m deep","m3",870,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over excavations for carting away ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Surplus material from excavations and/or stock piles on site to a dumping site to be located by the contractor","m3",444,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["BEDDING, BACKFILLING, ETC","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Filling from excavations including sifting and compaction to 93% MOD AASHTO density for backfilling to","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Pipe trenches ","m3",426,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Provide bedding (Blanket) from trench excavations in layers not exceeding 150mm thick, compacted to 93% MOD AASHTO density","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Selected granular material ","m3",102,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Selected fill material ","m3",337,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PIPEWORK","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["uPVC pipes Class 12 for use under ground in accordance with SABS 791 with uPVC couplings (Excavation, bedding material, back filling, compaction, etc. elsewhere)","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110mm Diameter pipe not exceeding 1m deep","m",1226,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra on uPVC pipes for flanged bitumen coated hot dipped galvanized steel fittings:","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100mm Bend, 22.5 degrees","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100mm Bend, 45 degrees","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100mm Bend, 90 degrees","No",14,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100mm Equal tee","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["100mm Flange adaptor","No",47,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Thrust blocks to 22.5 degree bends","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D13323*C13323","v":{"v":0,"d":"R0.00"}}]
["Size extreme 350 x 300 x 300mm high","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Thrust blocks to 45 degree bends","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Size extreme 500 x 250 x 400mm high","No",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Thrust blocks to 90 degree bends","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Size extreme 740 x 740 x 500mm high","No",14,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Thrust blocks to T-pieces","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Size extreme 650 x 325 x 400mm high","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sundries","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over excavation in earth for pipe trenches, chambers, etc for excavation in intermediate rock","m3",87,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over excavation in earth for pipe trenches, chambers, etc for excavation in hard rock","m3",87,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["IRRIGATION SLEEVES","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["uPVC sleeves laid in trenches (trenches elsewhere) ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["110mm Diameter sleeve pipes","m",699,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavate in earth and set excavated material aside for re-use as filling for:","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Sleeve trenches not exceeding 1m deep","m3",496,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Provide bedding from carted on material from commercial sources including sifting and compaction to 90% MOD AASHTO density for backfilling to","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Selected granular material","m3",99,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Provide main fill blanket from trench excavations in layers not exceeding 150mm thick, compacted to 95% MOD AASHTO density","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Selected fill material","m3",397,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Surplus material from the excavations spread and levelled over the site as directed","m3",99,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over excavations in 'earth' for sleeve trenches in 'intermediate rock'","m3",50,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over excavations in 'earth' for sleeve trenches in 'hard rock'","m3",50,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["GALVANIZED WATER TANKS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Approved hot dip galvanised steel sectional circular water tank, 6100mm diameter and 10000mm high with a capacity of 292 000 litres, formed of 6.4mm thick sheeting, cold rolled to the curvature required, a suction tank shall be fitted with a roof, a contents gauge, overflow pipe(s) and drainage facilities, the nominal diameter of the suction pipe shall suit the pump NPSH requirements, but shall not be less than 150 mm. The tank shall be fitted with a 50 mm ball float valve, a 50 mm drain valve piped to the floor drain outlet as well as a visual tank water level indicating device. An 80 mm overflow pipe shall also be drained to waste. A water-proving flow meter shall be fitted into the main pumped supply. This meter shall allow flow rates and pressures to be measured. There shall also be float switches inside each tank indicating if there is a high or low water condition. This alarm is raised on the Fire pump house annunciator panel and subsequently on the fire alarm panel in the central security/controls room. Float operated water level supervisory switches shall be provided for high and low water level alarms. The unit shall be single pole double throw snap-action, and enclosed in an oil resistant NEMA Type 2 drip proof, indoor rated housing. The housing cover shall be finished in red and secured with tamper resistant screws, which require a special key wrench for their removal. The electrical switch contacts shall be rated as follows and shall be connected by the Fire Detection and Alarm System Contractor to the central fire alarm panel: 125/250v AC 10.00 amps 6/12/24v DC 2.50 amps ","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Approved hot dip galvanised steel sectional circular water tank, 8074mm diameter and 6350mm high with a capacity of  419 000 litre, formed of 6mm thick sheeting, provided with two access openings covered with 3mm thick cover plates, two vermin and dust proof ventilators, two externally visible level indicators, two 100mm diameter inlet connection (roof), two 100mm diameter scour connections (wall), four 150mm diameter service connections (wall), four 40mm diameter control connections (roof), two 100mm diameter overflow connection (wall) internal dividing wall to separate tank in two equal compartments, including threaded inlet and outlet connections and overflow pipes, including 100mm flanged gate valve, including EPNS equilibrium float valve, including access opening covered with 3mm thick cover plate, sealing of joints, stiffeners, brackets, bolts, nuts, external ladder, completely erected with bottom of tank on concrete footings (elsewhere measured). All in accordance with the manufacturer's specifications and SABS CKS 114. ","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for testing of tanks by filling to maximum service level","Item",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["OFF-SITE VALVE CHAMBER AND WATER CONNECTION","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["VALVE CHAMBER","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavation in earth or compacted filling not exceeding 2m deep","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Valve chamber","m3",12,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Excavation in earth or compacted filling  exceeding 2m not exceeding 4m deep","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Valve chamber","m3",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D13387*C13387","v":{"v":0,"d":"R0.00"}}]
["Extra over excavations in earth for excavation in","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Soft rock","m3",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Hard rock","m3",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Extra over all excavations for carting away","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Surplus material from excavations and/or stock piles on site to a dumping site to be located by the contractor","m3",13,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Risk of collapse of excavations","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Ditto, but exceeding 1,5m deep and not exceeding 3m deep","m2",19,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Back excavation of vertical sides of excavation in earth, for working space, including backfilling compacted to 93% Mod AASHTO density","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Exceeding 1,5m and not exceeding 3m deep approximately 1,5m away from face of building including backfilling and compaction to 93% mod AASHTO density ","m2",19,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Approved G5 filling supplied and carted on by the Contractor, compacted in layers not exceeding 150mm to 95% Mod. AASHTO density","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Under solid floors ","m3",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Compaction of surfaces ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Compaction of ground surface under surface beds etc including scarifying for a depth of 150mm, breaking down oversize material, adding suitable material where necessary and compacting to 93% Mod AASHTO density","m2",6,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["UNREINFORCED CONCRETE CAST AGAINST EXCAVATED SURFACES ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["15MPa/19mm concrete","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Blinding under valve chamber","m3",0.3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["REINFORCED CONCRETE CAST AGAINST EXCAVATED SURFACES ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["25MPa/19mm concrete","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Valve chamber floor","m3",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["REINFORCED CONCRETE ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["25 MPa/19 mm concrete in","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Valve chamber walls","m3",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["ROUGH FORMWORK (DEGREE OF ACCURACY II)","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Rough formwork to sides","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Walls not exceeding 5m high","m2",45,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["REINFORCEMENT","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Fabric reinforcement","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Type 617 fabric reinforcement in concrete surface beds, slabs, walls, etc. ","m2",53,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Precast concrete cover slab","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["2800 x 2300 x 200mm Thick from 25Mpa/19mm reinforced concrete cover slab with mesh Ref 617 to top and bottom of slab with 560mm diameter access opening including additional Y12 reinforcement bars at bottom of opening in the direction of mesh wires. All edges to be chamfered 20 x 20mm, Type R10 hot dipped galvanized steel lifting hook to SANS 32 and 121, fixed to bottom reinforcement and cast into slab on each corner 150mm from edge of slab.","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PIPEWORK AND FITTINGS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Hot dipped galvanised screwed steel pipes and fittings as described","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"$f":"D13451*C13451","v":{"v":0,"d":"R0.00"}}]
["300mm Diameter Duroflo CI flange adaptor, PN 16","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["300mm Diameter pipe with puddle flange, flanged both ends, overall length 1095mm to Table 1600/3","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["300mm Diameter equal tee, flanged to Table 1600/3","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["300mm Diameter spool piece, flanged both ends, overall length 350mm to Table 1600/3","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["300mm Diameter Vosa wedge gate valve flanged PN 16, ball thrust collar, stainless steel trim, right hand closing non-rising spindle","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["300mm Diameter restrained flanged adaptor PN 16, with no 4 x M24 tie rods 350mm long","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["300mm Diameter spool piece, flanged one side, with puddle flange and restraining flange, overall length 1000mm, flanged to Table 1600/3","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["300mm Diameter 90 degree bend, flanged both ends, overall length 1220mm to Table 1600/3","No",4,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["300mm Diameter spool piece, flanged both ends, overall length 700mm to Table 1600/3","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["300mm Diameter blank flange to Table 1600/3","No",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["300 x 150mm Diameter reducer, flanged both ends, overall length 250mm to Table 1600/3","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150mm Diameter Vosa wedge gate valve flanged PN 16, ball thrust collar, stainless steel trim, right hand closing non-rising spindle","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150mm Diameter spool piece, flanged both ends, overall length 450mm to Table 1600/3","No",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["150mm Diameter Sensus WPD flow meter with hybrid register, PN 16","No",1,null,{"v":0,"d":"R0.00"}]
[]
["TOTAL EXTERNAL WATER SUPPLY",null,0,null,{"$f":"SUM(E13031:E13479)","v":{"v":0,"d":"0.00"}}]
[null,null,0]
["Demolitions ",null,null,{"v":0,"d":"R0.00"},{"$f":"E10476","v":{"v":0,"d":"R0.00"}}]
[]
["General Site Works, Roads and Paving",null,null,{"v":0,"d":"R0.00"},{"$f":"E11734","v":{"v":595000,"d":"R595,000.00"}}]
[]
["Yard Walls, Fencing, etc",null,null,{"v":0,"d":"R0.00"},{"$f":"E11944","v":{"v":0,"d":"R0.00"}}]
[]
["Landscaping ",null,null,{"v":0,"d":"R0.00"},{"$f":"E12262","v":{"v":1000000,"d":"R1,000,000.00"}}]
[]
["Stormwater Drainage",null,null,{"v":0,"d":"R0.00"},{"$f":"E12826","v":{"v":0,"d":"R0.00"}}]
[]
["Soil Drainage",null,null,{"v":0,"d":"R0.00"},{"$f":"E13030","v":{"v":0,"d":"R0.00"}}]
[]
["External Water Supply",null,null,{"v":0,"d":"R0.00"},{"$f":"E13480","v":{"v":0,"d":"R0.00"}}]
[]
["TOTAL SECTION 4 CARRIED TO FINAL SUMMARY",{"$nulls":3},{"$f":"SUM(E13482:E13495)","v":{"v":1595000,"d":"1,595,000.00"}}]
[]
["BILL NO 1","H2",0]
[]
["PROVISIONAL SUMS","H2",0]
[]
["SELECTED SUB CONTRACTS","H2",0]
[]
["The following provisional sums cover the complete supply and installation of material and equipment by firms of specialists to be selected sub-contractors. Provisional sums are nett and do not include for builders discount ",null,0]
[]
["The Contractor shall not be entitled to any loss in profit should any provisional sum or part thereof, irrespective of the amount be omitted ",null,0]
[]
["The Contractor may allow under the \"profit\" item for any profit he considers necessary. If the Contractor allows an amount for profit, this amount will be adjusted in direct proportion to the final value of the specialist work ",null,0]
[]
["Attendance on Selected Sub-contractors ","H3",0]
[]
["Each provisional sum in this bill is followed by an item under which the Contractor may allow for attendance on the specific Sub- contractor ",null,0]
[]
["The amounts of the items for \"Attendance\" are to allow for giving every facility to attending upon and making good in all trades after the Specialists have completed their work, for providing the use of all water, electricity, storage space for materials, etc. the use of general amenities, i.e.  latrines, etc., for the specialists and their workmen. For maintaining conduits, sleeve pipes, etc. in position during the building operations and providing the use of all ordinary scaffolding and plant. The Contractor is to leave erected scaffolding in position for the period required for work by the selected sub-contractors under this contract ",null,0]
[]
["--------------------------------- ",null,0]
[]
["ELECTRICAL INSTALLATION","H2",0]
[]
["Provide the sum of R336 800 000.00 (Three Hundred and Thirty Six Million Eight Hundred Thousand Rand) nett for Electrical Installation","Item",1,{"v":336800000,"d":"R336,800,000.00"},{"$f":"D13520*C13520","v":{"v":336800000,"d":"R336,800,000.00"}}]
[{"$nulls":4},{"$f":"D13521*C13521","v":{"v":0,"d":"R0.00"}}]
["Allow for profit if required ","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for attendance ","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["OPTICAL FIRE DETECTION INSTALLATION","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Provide the sum of R21 600 000.00 (Twenty One Million Six Hundred Thousand Rand) nett for Optical Fire Detection Installation","Item",1,{"v":21600000,"d":"R21,600,000.00"},{"v":21600000,"d":"R21,600,000.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for profit if required ","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for attendance ","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["FIRE PROTECTION INSTALLATION","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Provide the sum of R5 750 000.00 (Five Million Seven Hundred and Fifty Thousand Rand) nett for Fire Protection Installation","Item",1,{"v":5750000,"d":"R5,750,000.00"},{"v":5750000,"d":"R5,750,000.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for profit if required ","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for attendance ","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["ICT INSTALLATION","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Provide the sum of R41 800 000.00 (Forty One Million Eight Hundred Thousand Rand) nett for ICT Installation","Item",1,{"v":41800000,"d":"R41,800,000.00"},{"v":41800000,"d":"R41,800,000.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for profit if required.","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for attendance","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["NURSE CALL INSTALLATION","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Provide the sum of R14 400 000.00 (Fourteen Million Four Hundred Thousand Rand) nett for Nurse Call Installation","Item",1,{"v":14400000,"d":"R14,400,000.00"},{"v":14400000,"d":"R14,400,000.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for profit if required.","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for attendance","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["BUILDING MANAGEMENT SERVICE INSTALLATION","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Provide the sum of R8 100 000.00 (Eight Million One Hundred Thousand Rand) nett for Building Management Service Installation","Item",1,{"v":8100000,"d":"R8,100,000.00"},{"v":8100000,"d":"R8,100,000.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for profit if required.","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for attendance","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PUBLIC ADDRESS INSTALLATION","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Provide the sum of R1 600 000.00 (One Million Six Hundred Thousand Rand) nett for Public Address Installation","Item",1,{"v":1600000,"d":"R1,600,000.00"},{"v":1600000,"d":"R1,600,000.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for profit if required.","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for attendance","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SECURITY EQUIPMENT INSTALLATION","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Provide the sum of R15 700 000.00 (Fifteen Million Seven Hundred Thousand Rand) nett for Security Equipment Installation","Item",1,{"v":15700000,"d":"R15,700,000.00"},{"v":15700000,"d":"R15,700,000.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for profit if required.","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for attendance","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["HVAC DUCTING, DIFFUSION, AIR HANDLING UNITS AND VENTILATION INSTALLATION","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow the Amount of R67 350 000.00 (Sixty Seven Million Three Hundred and Fifty Thousand) nett for HVAC ducting, diffusion, Air handling units and Ventilation Installation ","Item",1,{"v":67350000,"d":"R67,350,000.00"},{"v":67350000,"d":"R67,350,000.00"}]
[{"$nulls":4},{"$f":"D13585*C13585","v":{"v":0,"d":"R0.00"}}]
["Allow for profit if required","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for attendance","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["CHILLED WATER INSTALLATION","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow the Amount of R33 200 000.00 (Thirty Three Million Two Hundred Thousand) nett for Chilled Water Installation ","Item",1,{"v":33200000,"d":"R33,200,000.00"},{"v":33200000,"d":"R33,200,000.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for profit if required","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for attendance","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["MEDICAL GAS INSTALLATION","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow the Amount of R R16 700 000.00 (Sixteen Million Seven Hundred Thousand Rand) nett for Medical Gas Installation","Item",1,{"v":16700000,"d":"R16,700,000.00"},{"v":16700000,"d":"R16,700,000.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for profit if required","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for attendance","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["LIFT AND ESCALATOR INSTALLATION ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow the Amount of R17 400 000.00 (Seventeen Million Four Hundred Thousand Rand) nett for Lift and Escalator Installation","Item",1,{"v":17400000,"d":"R17,400,000.00"},{"v":17400000,"d":"R17,400,000.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for profit if required","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for attendance","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["KITCHEN INSTALLATION ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow the Amount of R3 300 000.00 (Three Million Three Hundred Thousand Rand) nett for Kitchen Installation","Item",1,{"v":3300000,"d":"R3,300,000.00"},{"v":3300000,"d":"R3,300,000.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
[" Allow for profit if required","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for attendance","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["LAUNDRY INSTALLATION ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow the Amount of R8 800 000.00 (Eight Million Eight Hundred Thousand Rand) nett  for Laundry Installation","Item",1,{"v":8800000,"d":"R8,800,000.00"},{"v":8800000,"d":"R8,800,000.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for profit if required","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for attendance","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["COLD ROOM INSTALLATION ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow the Amount of R1 000 000.00 (One Million Rand) nett for Cold Room Installation","Item",1,{"v":1000000,"d":"R1,000,000.00"},{"v":1000000,"d":"R1,000,000.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
[" Allow for profit if required.","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for attendance","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["MORTUARY REFRIGERATION ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow the Amount of R1 300 000.00 (One Million Three Hundred Thousand Rand) nett for Mortuary Refrigeration ","Item",1,{"v":1300000,"d":"R1,300,000.00"},{"v":1300000,"d":"R1,300,000.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for profit if required","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for attendance","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["STERILIZATION EQUIPMENT ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow the Amount of R4 650 000.00 (Four Million Six Hundred and Fifty Thousand Rand) nett for Sterilization Equipment ","Item",1,{"v":4650000,"d":"R4,650,000.00"},{"v":4650000,"d":"R4,650,000.00"}]
[{"$nulls":4},{"$f":"D13649*C13649","v":{"v":0,"d":"R0.00"}}]
["Allow for profit if required","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for attendance","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["WASTE MANAGEMENT ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow the Amount of R800 000.00 (Eight Hundred Thousand Rand) nett for Waste Management ","Item",1,{"v":800000,"d":"R800,000.00"},{"v":800000,"d":"R800,000.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for profit if required","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for attendance","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["RENAL WATER","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow the Amount of R500 000.00 (Five Hundred Thousand Rand) nett for Boiler Installation","Item",1,{"v":500000,"d":"R500,000.00"},{"v":500000,"d":"R500,000.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for profit if required","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for attendance","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["BOREHOLE INSTALLATION ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow the Amount of R750 000.00 (Seven Hundred and Fifty Thousand Rand), nett for borehole installation ","Item",1,{"v":750000,"d":"R750,000.00"},{"v":750000,"d":"R750,000.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for profit if required","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for attendance ","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SOFT LANDSCAPING AND IRRIGATION","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow the Amount of R11 000 000.00 (Eleven Million Rand) nett for Soft Landscaping and Irrigation ","Item",1,{"v":11000000,"d":"R11,000,000.00"},{"v":11000000,"d":"R11,000,000.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for profit if required","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for attendance","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["LANDSCAPE MAINTENANCE ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow the Amount of R1 500 000.00 (One Million Five Hundred Thousand Rand) nett for Landscape Maintenance ","Item",1,{"v":1500000,"d":"R1,500,000.00"},{"v":1500000,"d":"R1,500,000.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for profit if required","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for attendance ","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["FIREPROOFING","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow the Amount of R1 300 000.00 (One Million Three Hundred Thousand Rand) nett for Fireproofing and sealing","Item",1,{"v":1300000,"d":"R1,300,000.00"},{"v":1300000,"d":"R1,300,000.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for profit if required","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for attendance","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TRAINING","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow the Amount of R12 000 000.00 (Twelve Million Rand) nett for Training","Item",1,{"v":12000000,"d":"R12,000,000.00"},{"v":12000000,"d":"R12,000,000.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for profit if required","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for attendance","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["COMMUNITY LIAISON OFFICER","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow the Amount of R1 000 000.00 (One Million Rand) nett for monthly payment of the Community Liaison Officer ","Item",1,{"v":1000000,"d":"R1,000,000.00"},{"v":1000000,"d":"R1,000,000.00"}]
[{"$nulls":4},{"$f":"D13713*C13713","v":{"v":0,"d":"R0.00"}}]
["Allow for profit if required","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for attendance ","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TRAFFIC LIGHTS / SIGNALIZATION","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Provide the sum of R1 500 000.00 (One Million Five Hundred Thousand Rand) nett for Traffic Lights / Signalization","Item",1,{"v":1500000,"d":"R1,500,000.00"},{"v":1500000,"d":"R1,500,000.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
[" Allow for profit if required","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for attendance","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["AUDITORIUM AUDIO VISUAL","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Provide the sum of R1 000 000.00 (One Million Rand) nett for Auditorium Audio Visual","Item",1,{"v":1000000,"d":"R1,000,000.00"},{"v":1000000,"d":"R1,000,000.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for profit if required ","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for attendance","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["AUDITORIUM SEATING","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Provide the sum of R500 000.00 (Five Hundred Thousand Rand) nett for Auditorium Seating","Item",1,{"v":500000,"d":"R500,000.00"},{"v":500000,"d":"R500,000.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for profit if required ","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for attendance","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["FALL PROTECTION","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Provide the sum of R3 600 000.00 (Three Million Six Hundred Thousand Rand) nett for Fall Protection","Item",1,{"v":3600000,"d":"R3,600,000.00"},{"v":3600000,"d":"R3,600,000.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for profit if required ","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for attendance","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["ALUMINIUM DOORS, CURTAIN WALLS, ROLLER SHUTTERS AND SPECIALIST DOORS INCLUDING IRONMONGERY, AUTOMATIC DOOR CLOSERS AND ACCESS CONTROL PROVISION","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Provide the sum of R17 500 000.00 (Seventeen Million Five Hundred Thousand Rand) nett for Aluminium Doors, Curtain Walls, Roller Shutters, Specialist Doors including Ironmongery, automatic Door Closers and Access Control Provision ","Item",1,{"v":17500000,"d":"R17,500,000.00"},{"v":17500000,"d":"R17,500,000.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for profit if required ","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for attendance ","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["ALUMINIUM LASER CUT AND GLASS SUN SCREENS INCLUDING STEEL SUPPORT STRUCTURES ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Provide the sum of R20 600 000.00 (Twenty Million Six Hundred Thousand Rand) nett for Aluminium Laser Cut and Glass Sun Screens Including Steel Support Structures ","Item",1,{"v":20600000,"d":"R20,600,000.00"},{"v":20600000,"d":"R20,600,000.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for profit if required ","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for attendance ","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["HOSPITAL STREET GLASS WALL FACADE AND ROOF INCLUDING STEEL SUPPORT STRUCTURE AND RAINWATER DISPOSAL ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Provide the sum of R22 000 000.00 (Twenty Two Million Rand) nett for Hospital Street Glass Wall Façade and Roof Including Steel Support Structure and Rainwater Disposal ","Item",1,{"v":22000000,"d":"R22,000,000.00"},{"v":22000000,"d":"R22,000,000.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for profit if required ","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for attendance ","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["PNEUMATIC TUBE SYSTEM - MECHANICAL INSTALLATION  ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Provide the sum of R22 000 000.00 (Twenty Two Million Rand) nett for Pneumatic Tube System Mechanical Installation ","Item",1,{"v":22000000,"d":"R22,000,000.00"},{"v":22000000,"d":"R22,000,000.00"}]
[{"$nulls":4},{"$f":"D13777*C13777","v":{"v":0,"d":"R0.00"}}]
["Allow for profit if required ","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for attendance ","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TOTAL SECTION 5 CARRIED TO FINAL SUMMARY",null,0,null,{"$f":"SUM(E13498:E13781)","v":{"v":717000000,"d":"717,000,000.00"}}]
[null,null,0,null,{"v":0,"d":"R0.00"}]
[]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SECTION NO. 6","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["BILL NO 1","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["HEALTH TECHNOLOGY EQUIPMENT PROVISION ","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["SELECTED SUB CONTRACTS","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The following provisional sums cover the complete supply and installation of material and equipment by firms of specialists to be selected sub-contractors. Provisional sums are nett and do not include for builders discount ",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The Contractor shall not be entitled to any loss in profit should any provisional sum or part thereof, irrespective of the amount be omitted ",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The Contractor may allow under the \"profit\" item for any profit he considers necessary. If the Contractor allows an amount for profit, this amount will be adjusted in direct proportion to the final value of the specialist work ",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Attendance on Selected Sub-contractors ","H3",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Each provisional sum in this bill is followed by an item under which the Contractor may allow for attendance on the specific Sub- contractor ",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["The amounts of the items for \"Attendance\" are to allow for giving every facility to attending upon and making good in all trades after the Specialists have completed their work, for providing the use of all water, electricity, storage space for materials, etc. the use of general amenities, i.e.  latrines, etc., for the specialists and their workmen. For maintaining conduits, sleeve pipes, etc. in position during the building operations and providing the use of all ordinary scaffolding and plant. The Contractor is to leave erected scaffolding in position for the period required for work by the selected sub-contractors under this contract ",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["--------------------------------- ",null,0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["HEALTH TECHNOLOGY EQUIPMENT","H2",0,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow the Amount of R803 500 000.00 (Eight Hundred and Three Million Five Hundred Thousand Rand) nett for Health Technology Equipment ","Item",1,{"v":803500000,"d":"R803,500,000.00"},{"v":803500000,"d":"R803,500,000.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for profit if required ","%IT",1,null,{"$f":"D13812*C13812","v":{"v":0,"d":"R0.00"}}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["Allow for limited attendance. No installation, loose equipment and furniture only. Delivery after practical completion.","%IT",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},{"v":0,"d":"R0.00"}]
["TOTAL SECTION 6 CARRIED TO FINAL SUMMARY",null,0,null,{"$f":"SUM(E13783:E13815)","v":{"v":803500000,"d":"803,500,000.00"}}]
[]
["SECTION 1 - PRELIMINARIES ",null,null,{"v":0,"d":"R0.00"},{"$f":"E970","v":{"v":0,"d":"R0.00"}}]
[]
["SECTION 2 - BUILDING WORK",null,null,{"v":0,"d":"R0.00"},{"$f":"E10216","v":{"v":1050000,"d":"R1,050,000.00"}}]
[]
["SECTION 3 - THERMAL ACTIVATED BUILDING SYSTEM (PROVISIONAL)",null,null,{"v":0,"d":"R0.00"},{"$f":"E10378","v":{"v":0,"d":"R0.00"}}]
[]
["SECTION 4 - EXTERNAL WORKS (PROVISIONAL)",null,null,{"v":0,"d":"R0.00"},{"$f":"E13496","v":{"v":1595000,"d":"R1,595,000.00"}}]
[]
["SECTION 5 - PROVISIONAL AMOUNTS",null,null,{"v":0,"d":"R0.00"},{"$f":"E13782","v":{"v":717000000,"d":"R717,000,000.00"}}]
[]
["SECTION 6 - HEALTH TECHNOLOGY ",null,null,{"v":0,"d":"R0.00"},{"$f":"E13816","v":{"v":803500000,"d":"R803,500,000.00"}}]
[]
["SUB TOTAL ",null,0,null,{"$f":"SUM(E13817:E13829)","v":{"v":1523145000,"d":"1,523,145,000.00"}}]
[]
["ALLOWANCES","H3",0]
[]
["Allow the Amount of R90 000 000.00 (Ninety Million Rand) for Contingencies to be used at the discretion of the Employer, or to be deducted in whole or in part if not required","Item",1,{"v":90000000,"d":"R90,000,000.00"},{"v":90000000,"d":"R90,000,000.00"}]
[]
["Allow the Amount of R235 000 000.00 (Two Hundred and Thirty Five Million Rand) for Escalation to be adjusted accordingly to the conditions of contract","Item",1,{"v":235000000,"d":"R235,000,000.00"},{"v":235000000,"d":"R235,000,000.00"}]
[]
["SUB TOTAL (EXCLUDING VAT @ 15%)",null,0,null,{"$f":"E13830+E13834+E13836","v":{"v":1848145000,"d":"1,848,145,000.00"}}]
[{"$nulls":4},{"$f":"D13839*C13839","v":{"v":0,"d":"0.00"}}]
["VAT @ 15%","TAX",{"v":0.15,"d":"15%"},null,{"$f":"E13838*0.15","v":{"v":277221750,"d":"277,221,750.00"}}]
[]
["TOTAL (INCLUDING VAT @ 15%)",{"$nulls":3},{"$f":"E13838+E13840","v":{"v":2125366750,"d":"2,125,366,750.00"}}]