{"text_format":"3","workbook":"xls","n_sheets":23,"sheets":["1. Preliminary and General","2. Provisional Sums","3. SHREQ","4. EMS","4B Quality","5. Dayworks","6. Civil - Site Clearance","7. Civil - Earthworks","8. Civil - Concrete","9. Civil - Precast Concrete","10. Civil - Structural Steel","11. Pipeline - Site Clearance","12. Pipeline - Earthwork & Bed","13.Pipeline-Pipes and Specials","14.Pipelines-PipeSpecials M & V","15.Pipeline - Pipeline Sundries","16.Pipeline-Cathodic Protect","17. Mechanical Header","18. Mechanical Refurb","19. Access Road ","20. SED","21.Summary","Sheet1"],"not_rendered":{"images":41,"external_links":3,"defined_names":21},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"1. Preliminary and General","index":0,"n_rows":213,"n_cols":7,"rows_kept":213,"merged":[[1,7,2,7],[5,1,6,1],[50,0,50,2],[52,0,52,5],[89,0,89,2],[91,0,91,5],[151,0,151,2],[153,0,153,5],[212,0,212,5]],"flags":["formulas_cached_only"]}
[null,null,"Lethabo Pump Station: ",{"$nulls":3},"SANS 1200A"]
[null,null,"Header upgrade at Lethabo Pumping Station",{"$nulls":3},"Section 1 :  P&G Time Related"]
[]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate","Amount"]
[]
[null,"SANS 1200A","SECTION 1:  PRELIMINARY & GENERAL"]
[null,null,"FIXED CHARGES"]
[]
[1.1,"8.3.1","Contractual Requirements","Sum",1]
[]
[null,"8.3.2","Establishment of Facilities on Site"]
[]
[1.2,"8.3.2.1","Facilities for Engineer  (SANS 1200AB)"]
[]
["1.2.1","PSAB 3.2 PSAB 5.2","Provision of Office for the Engineer's Representative ","Sum",1]
[]
["1.2.2","PSAB 4.2","Provision of survey equipment","Sum",1]
[]
["1.2.3","8.3.2.1(b)","4 Covered parking bays as directed by the Engineer","Sum",1]
[]
["1.2.4","8.3.2.1(c)","Construction name boards x 2","No.",1]
[]
["1.2.5","8.3.2.1(d)","Survey assistant and materials","Sum",1]
[]
[1.3,"8.3.2.2","Facilities for Contractor"]
[]
["1.3.1","8.3.2.2\n(a)(b)(c)","Offices, storage sheds, fencing, workshops, laboratories, etc.","Sum",1]
[]
["1.3.2","8.3.2.2(e)","Ablution and latrine facilities","Sum",1]
[]
["1.3.3","8.3.2.2(f)","Tools and equipment","Sum",1]
[]
["1.3.4","8.3.2.2(g)","Water supplies, electric power and communications","Sum",1]
[]
[1.4,"PSA 8.8.7","Dealing with water","Sum",1]
[]
[1.5,"8.3.3","Other fixed charge obligations, including setting out of works, security of contractor's plant & personnel","Sum",1]
[]
[1.6,"8.3.4","Remove all site establishment on completion","Sum",1]
[]
[1.7,"8.3.5","Security of Contractor's plant","Sum",1]
[]
[1.8,"PSA 8.3.5","Health and Safety Plan"]
[]
[null,null,"Provide a Health and Safety Plan which comply to all the requirements of the OHS Act for the duration of the Contract","Sum",1]
[]
[1.9,"PSA 8.3.6","Environmental Management Plan"]
[]
["1.9.1",null,"Comply with all requirements of the Environmental Management Plan and RoD for the duration of the Contract.","Sum",1]
[]
["Total Carried forward "]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate","Amount"]
["Total  brought Forward  "]
[{"v":1.1,"d":"1.10"},null,"Accommodation of traffic"]
[]
["1.10.1","PSA 8.8.2  and 8.6 (k)    ","The supply, maintaining and removal of traffic control devices, road signs, canalisation of traffic, barricades, including New Jersey type, warning signs, including signs for construction vehicles and road markings","Sum",1]
[]
[1.11,null,"HIV / AIDS awareness"]
[]
["1.11.1",null,"Conduct HIV/AIDS awareness programme workshops on site for not less than 90% of the workers inclusive of all direct and indirect costs","Sum",1]
[]
["1.11.2",null,"Provide and maintain condom dispenser","Sum",1]
[]
["1.11.3",null,"Provide and maintain HIV/AIDS awareness posters","Sum",1]
[]
["1.11.4",null,"Provide information regarding voluntary testing of construction workers and counselling, support and care in a monthly report.","Sum",1]
[]
[1.12,null,"Quality Control"]
[]
["1.12.1",null,"The sum shall cover the cost of all activities necessary to comply with all requirements of the specified quality control system as per PS 4","Sum",1]
[]
[1.13,null,"As Builts"]
[]
["1.13.1","PSA 8.16","The provision of detailed as-builts drawings of the completed works as per specification.","Sum",1]
[]
["1.14",null,"Access to spoil sites"]
[]
["1.14.1","PS 17","The identification of spoil sites for the disposal of unsuitable or suplus excavation materials, negotiations and agreement with relevant owners and/or authorities and the provision of access to designated spoil sites ","Sum",1]
[]
[1.15,"PSA 8.10","Provision of crane with about 50m arm reach for working above the sasol pipeline in order to protect it throughout the construction period of the header upgrading.","Sum",1]
[]
[]
[]
[]
[]
[1.17,null,"Shoring"]
[]
["1.17.1",null,"The sum shall cover the cost of the design, geotechnical studies and erection of a suitable shoring system for an approximate length of 350m and a varying height of 8 - 12m","Sum",1]
[]
["Total Carried forward "]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate","Amount"]
["Total Brought Forward  "]
[1.18,"SABS 1200A","\nTIME RELATED ITEMS"]
[]
["1.18.1","8.4.1","Contractual Requirements","Sum",1]
[]
["1.18.1.1","8.4.2","Operate and maintain facilities on Site"]
[]
["1.18.2","8.4.2","Facilities for Engineer for duration of Contract (SABS 1200AB)"]
[]
["1.18.2.1","PSAB 3.2 PSAB 5.2","Provision of office for the Engineer's representative","Sum",1]
[]
["1.18.2.2","PSAB 4.2","Provision of survey equipment","Sum",1]
[]
["1.18.2.3","8.3.2.1(b)","4 Covered parking bays as directed by the Engineer","Sum",1]
[]
["1.18.2.4","8.4.2.1(c)","Name Board as shown on Sketch bound to back of document","Sum",1]
[]
["1.18.2.5","8.4.2.1(d)","Provision of survey assistants","Sum",1]
[]
["1.18.3","8.4.2.2","Facilities for Contractor"]
[]
["1.18.3.1","8.4.2.2\n(a)(b)(c)","Offices, storage sheds, fencing, workshops, laboratories, etc.","Sum",1]
[]
["1.18.3.2","8.4.2.2(e)","Ablution and latrine facilities","Sum",1]
[]
["1.18.3.3","8.4.2.2(f)","Tools and equipment","Sum",1]
[]
["1.18.3.4","8.4.2.2(g)","Water supplies, electric power and communications","Sum",1]
[]
[1.19,"PSA 8.8.7","Dealing with water","Sum",1]
[]
[{"v":1.2,"d":"1.20"},"8.4.3","Supervision for duration of construction","Sum",1]
[]
[1.21,"8.4.4","Company and head office overhead costs","Sum",1]
[]
[1.22,"8.4.5","Other time related charges, including security of contractor's plant & personnel","Sum",1]
[]
[1.23,null,"Accommodation of traffic"]
[]
["1.23.1","PSA 8.8.2  and 8.6 (k)    ","The supply, maintaining and removal of traffic control devices, road signs, canalisation of traffic, barricades, including New Jersey type, warning signs, including signs for construction vehicles and road markings","Sum",1]
{"$rows_empty":20}
["Total Carried forward "]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate","Amount"]
["Total Brought Forward  "]
[]
[1.24,null,"As Builts"]
[]
["1.24.1","PSA 8.16","The provision of detailed as-builts drawings of the completed works","Sum",1]
[]
[1.25,null,"Access to Spoil Sites"]
[]
["1.25.1","PS 17","Sum associated with identification, negotiations and access to designated spoil sites for disposal of surplus spoil material","Sum",1]
[]
[1.26,null,"Temporary Works"]
[]
["1.26.1","8.8.1","Access to works including all temporary roads, excavations and ramps, etc.","Sum",0]
[]
[1.27,null,"Other costs"]
[]
["1.27.1","PSA 8.8.8","Discontinue operations (where instructed by the Engineer due to lack of access) and transfer plant,equipement and labour"]
[]
["1.27.1.1",null,"De-establishing and Re-establishing after phase 1","Sum",1]
[]
["1.27.1.2",null,"De-establishing and Re-establishing after phase 2","Sum",1]
[]
["1.27.1.3",null,"De-establishing and Re-establishing after phase 3","Sum",1]
[]
[]
[1.28,"PSA 8.8.11","Standing time costs ","Days",40]
[]
[1.29,"PSA 8.8.12","Carry out operations in a confined and reduced working strip width","m",200]
[]
[{"v":1.3,"d":"1.30"},"8.8.4","Existing services"]
[]
["1.31.1",null,"a) Supply or hire specialist equipment for the detection of underground services","Sum",1]
[]
["1.31.2",null,"b) The use of equipment referred to in item (a) above","Sum",1]
[]
["1.31.3",null,"c) Excavation by hand in soft material to expose services","Sum",1]
[]
["1.31.4",null,"d) Temporary protection","Sum",1]
[]
[1.32,"PSA 8.10","Provision of crane with about 50m arm reach for working above the Sasol Pipeline in order to protect it throughout the construction period of the header upgrading.","Sum",1]
[]
[]
[1.33,null,"Generate & Provide as Build Drawings  ","Set of ",3]
[]
[1.34,null,"Geotechnical Engineer appointment and studies","Sum",1]
{"$rows_empty":14}
["Total Section 1: Carried Forward to Summary"]

{"sheet":"2. Provisional Sums","index":1,"n_rows":88,"n_cols":7,"rows_kept":88,"merged":[[52,0,52,2],[54,0,54,5],[87,0,88,5],[87,6,88,6]],"flags":["formulas_cached_only"]}
[null,null,"Lethabo Pump Station: ",{"$nulls":3},"Section 2: Provisional Sums"]
["Contract No.:",null,"Header upgrade at Lethabo Pumping Station"]
["Description:"]
[]
["Item ","Payment","Description","Unit","Qty","Rate","Amount"]
["No.","Refers"]
[]
[null,"SANS 1200A","SECTION 2:  PROVISIONAL SUMS, PRIME COSTS AND OTHER COSTS"]
[]
[2,"SANS","Provisional Sums allowed for by the Client"]
[null,"1200A"]
[2.1,null,"Relocation of existing services"]
[]
["2.1.1","8.5 (b)(1)","Provisional sum for the relocation of existing services (water mains, overhead or underground electrical, etc) by services utilities","Prov. Sum",1,{"v":100000,"d":"100,000.00"},{"v":100000,"d":"100,000.00"}]
[]
["2.1.2","8.5 (b)(2)","Contractors mark-up on Item 4.1.1","%",{"v":100000,"d":"100,000.00"}]
[]
[2.2,null,"Additional surveys"]
[]
["2.2.1","8.5 (b)(1)","Additional topographical surveys and underground service detection by nominated specialist as ordered by Engineer","Prov. Sum",1,{"v":100000,"d":"100,000.00"},{"v":100000,"d":"100,000.00"}]
[]
["2.2.2","8.5 (b)(2)","Contractors mark-up on Item 4.2.1","%",{"v":100000,"d":"100,000.00"}]
[]
[2.3,null,"Office equipment"]
[]
["2.3.1","8.5 (a)","Provisional Sum for supply of office equipment for Engineer's Representative Offices not included under Item 2 of Section 1 of Bill of Quantties","Prov. Sum",1,{"v":50000,"d":"50,000.00"},{"v":50000,"d":"50,000.00"}]
[]
["2.3.2","8.5 (b)(2)","Contractor's mark up on Item 4.3.1","%",{"v":50000,"d":"50,000.00"}]
[]
[2.4,null,"Dealing with Sasol Pipeline"]
[]
["2.4.1","PSA 8.10","Provisional Sum for protection and recoating of a section of Sasol pipeline","Prov. Sum",1,{"v":1500000,"d":"1,500,000.00"},{"v":1500000,"d":"1,500,000.00"}]
[]
["2.4.2",null,"Contractor's mark up on Item 4.4.1","%",{"v":1500000,"d":"1,500,000.00"}]
[]
[2.5,null,"Dealing with pipes already installed"]
["2.5.1","PSA 8.10","Provisional Sum for exposing and assessment of already installed pipes including X-ray and backfilling accordingly","Prov. Sum",1,{"v":1500000,"d":"1,500,000.00"},{"v":1500000,"d":"1,500,000.00"}]
[]
[null,null,"Contractor's mark up on Item 4.5.1","%",{"v":1500000,"d":"1,500,000.00"}]
[]
[2.6,null,"Non Destructive testing"]
[]
["2.6.1","8.5 (a)","Provisional sum for additional non-destructive pipeline testing as directed by Engineer ","Prov. Sum",1,{"v":100000,"d":"100,000.00"},{"v":100000,"d":"100,000.00"}]
[]
["2.6.2","8.5 (b)(2)","Contractors mark-up on Items 4.6.1","%",{"v":100000,"d":"100,000.00"}]
[]
[2.7,null,"Existing B5 and B11 Pipelines"]
[]
["2.7.1","PSA 8.10","Provisional Sum for locating of verification existing B5 and B11 pipelines air valves including dealing with shutdowns ","Prov. Sum",1,{"v":1500000,"d":"1,500,000.00"},{"v":1500000,"d":"1,500,000.00"}]
[]
["2.7.2",null,"Contractors mark-up on Item 4.7.1","%",{"v":1500000,"d":"1,500,000.00"}]
[]
["Total brought forward "]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate","Amount"]
["Total Carried Forward  "]
[]
[2.8,null,"Additional Geotechnical Investigation"]
[]
["2.8.1","PSA 8.10","Additional Geotech for material on site","Prov Sum",1,{"v":300000,"d":"300,000.00"},{"v":300000,"d":"300,000.00"}]
[]
["2.8.2",null,"Contractors mark-up on Item 4.8.1","%",{"v":300000,"d":"300,000.00"}]
[]
[2.9,null,"Refurbishment of pipes and specials"]
[]
["2.9.1","PSA 8.10","Allow Provisional Sum for refurbishment of specials and pipes on site","Prov \nSum",1,{"v":2300000,"d":"2,300,000.00"},{"v":2300000,"d":"2,300,000.00"}]
[]
["2.9.2",null,"Contractors mark-up on Item 4.9.1","%",{"v":2300000,"d":"2,300,000.00"}]
[]
[{"v":2.1,"d":"2.10"},null,"Design, Supply, Install,  Commissioning of Electrical cables, Switched and Equipemnt etc. as per electrical system specification  -RW10396363/21/ELEC-SPEC: ELECTRICAL SYSTEM SPECIFICATION","Prov Sum ",1,{"v":4000000,"d":"4,000,000.00"},{"v":4000000,"d":"4,000,000.00"}]
[]
[2.11,null,"Design, Supply, Install,  Commissioning of Automation network,cables  and Equipemnt etc. as per Automation System Specification  -RW10396363/21/Auto/Spec: Automation System Specification ","Prov Sum ",1,{"v":3000000,"d":"3,000,000.00"},{"v":3000000,"d":"3,000,000.00"}]
[]
[null,null,"Design, supply, install and put into operation drainage pump system and pump cooling water system as per Mechanical System Specification  -RW10396363/21/Mech-Refurb/Spec: Mechanical Specification","Prov Sum",1]
[]
[12.12,null,"SURGE TANK "]
[]
[null,null,"Transport and deliver dismentled tank & pipes  at Rand Water Emhlangeni Pipe RW10396363/21/Mech/Spec:Mechanical Specification Clause  2.7.1","Prov Sum ",1,{"v":100000,"d":"100,000.00"},{"v":100000,"d":"100,000.00"}]
["12.12.1",null,"Design, Supply, Manufacture, Deliver and install new Surge Tank complete with associated piping and fittings as per Rand Water document RW10396363/21/Mech/Spec:Mechanical Specification Clause  2.7.3","Prov Sum ",1,{"v":1000000,"d":"1,000,000.00"},{"v":1000000,"d":"1,000,000.00"}]
[]
["12.12.2",null,"Design and construct the foundation for the tank, chambers, valves and associated pipes etc.  as per Rand Water document RW10396363/21/Mech/Spec:Mechanical Specification Clause  2.7.3","Prov Sum ",1,{"v":500000,"d":"500,000.00"},{"v":500000,"d":"500,000.00"}]
[]
["12.12.3",null,"Manufacture , supply, deliver  and install new valves complete with fittings for the surge tanks RW10396363/21/Mech/Spec:Mechanical Specification Clause  2.7.3","Prov Sum ",1,{"v":10000000,"d":"10,000,000.00"},{"v":10000000,"d":"10,000,000.00"}]
[]
[]
[]
[]
[]
["Total Section 2: Carried Carried Forward to Summary",{"$nulls":5},{"v":26050000,"d":"26,050,000.00"}]

{"sheet":"3. SHREQ","index":2,"n_rows":58,"n_cols":7,"rows_kept":58,"merged":[[57,0,57,5]],"flags":["formulas_cached_only"]}
[{"$nulls":6},"Section 3:  OH&S and Environment"]
["Contract No.:",null,"Lethabo Pump Station: "]
["Description:",null,"Header upgrade at Lethabo Pumping Station"]
[]
["Item ","Payment","Description","Unit","Qty","Rate","Amount"]
["No.","Refers"]
[null,null,"SECTION 3 :  OCCUPATIONAL HEALTH AND SAFETY AND ENVIRONMENT"]
[{"$nulls":4},"``"]
[3.1,"PSA 8.11","OCCUPATIONAL HEALTH AND SAFETY"]
[]
["3.1.1"," ","Preparation of the Contractor's site specific Health and Safety Plan","Sum",1]
[]
["3.1.2",null,"Principal Contractor's initial obligations in respect of the Occupational Health and Safety Act and Construction Regulations","Sum",1]
[]
["3.1.3",null,"Principal Contractor's time related obligations in respect of the Occupational Health and Safety Act and Construction Regulations","Sum",1]
[]
["3.1.4",null,"Provision of Personal Protective Equipment (PPE)","Sum",1]
[]
["3.1.5",null,"Provision of a full-time Construction Health and Safety Officer","Sum",1]
[]
["3.1.6",null,"Cost of medical certificates and medical surveillance"]
[]
["3.1.6.1",null,"(a) Initial (baseline) medical examinations","Sum",1]
[]
["3.1.6.2",null,"(b) Periodic and exit examinations","Sum",1]
[]
["3.1.6.3",null,"(c) Exit examinations","Sum",1]
[]
["3.1.7",null,"Induction training","Sum",1]
[]
["3.1.8",null,"Provision of First Aid Boxes to GSR requirements and other emergency safety equipment such as fire extinguishers.","Sum",1]
[]
["3.1.9",null,"Transportation of Workers","Sum",1]
[]
["3.1.10",null,"Welfare Facilities","Sum",1]
[]
["3.1.11",null,"Occupational Hygiene Surveys","Sum",1]
[]
["3.1.12",null,"Training","Sum",1]
[]
["3.1.13",null,"Security requirements including the security risk assessment (before site establishment)","Sum",1]
[]
["3.1.14",null,"Employee wellness programs","Sum",1]
[]
["3.1.15",null,"Drug and Alcohol Testing, Policies and Procedures","Sum",1]
[]
["3.1.16",null,"Barricading","Sum",1]
[]
["3.1.17",null,"Safety notices and signs","Sum",1]
[]
["3.1.18",null,"SHE  Incentives","Sum",1]
[]
["3.1.19",null,"Compliance With Covid -19 Requirements As Per The She Specification","Sum",1]
[]
["3.1.20",null,"Adequate ventilation and lighting during construction","Sum",1]
[]
["3.1.21",null,"Submission of the Health and Safety File (hard and soft copies)","Sum",1]
["Total Section 3:  Carried Forward to Summary"]

{"sheet":"4. EMS","index":3,"n_rows":58,"n_cols":9,"rows_kept":58,"merged":[[10,0,15,0],[11,3,15,3],[11,4,15,4],[20,3,26,3],[20,4,26,4],[27,0,30,0],[27,3,29,3],[27,4,29,4],[52,0,52,6],[53,2,53,5],[54,2,54,5],[55,2,55,5],[56,2,56,5],[57,0,57,5]],"flags":["formulas_cached_only"]}
[{"$nulls":6},"Section 4:  Environment"]
[null,null,"Lethabo Pump Station: "]
[null,null,"Header upgrade at Lethabo Pumping Station"]
[]
["Item ","Payment","Description","Unit","Qty","Rate","Amount"]
["No.","Refers"]
[]
[4,"PSA 8.3.14","ENVIRONMENT"]
[4.1,9.1,"Administrative requirements as per environmental specification.                                             • Understanding of compliance\n• Preparation of environmental file and work program approval.\n• Preparations of method statements (management of all waste, Keeping the site clean and weed free, final clean up of site and campsite). \n• Maintaining of auditing of site compliances\n• Reporting of environmental incidence\n• Signing off of work for payment \n• Emergency preparedness retainement for external services\n• Programme scheduling details of administrative matters:\n","Sum",1,{"$nulls":3},"Is this not a duplication for name board?"]
[]
[4.2,9.2,"Emergency preparedness funding"]
[null,null,"a)          Provision for bee, snake and other fauna removal","Sum",1]
[null,null,"b)          Provision for hydrocarbon spillages that require intervention from professional clean up provider"]
[null,null,"c)           Provision to clean up sewage spillages"]
[null,null,"d)          Equipment for fire fighting"]
[null,null,"e)          Call out of fire department"]
[4.3,"9.1.4","Environmental awareness and training "]
[null,null,"The rate for this item shall include costs for inductions and environmental awareness and training","Sum",1]
[4.4,9.2,"Social integration of the project to the public "]
[null,null,"The rate for this item shall include costs for establishment of construction campsite and working areas","Sum",1]
[4.5,9.3,"Establishment of site camp and works area.","Sum",1]
[null,null,"Signage The rate for this item must cover all expenses incurred in preparing signage at the entrance of the site offices indicating the following information "]
[null,null,"·        The contractor’s contact numbers"]
[null,null,"·        ECO details "]
[null,null,"·        Emergency numbers and provision for: – snake removal, bee removal, fire, large hydrocarbon spillages, sewerage spillages"]
[null,null,"Signage measuring a minimum of 30mmx30mm must also be made available for no go areas."]
[4.6,"9.3.4 to 9.3.4.2","Barricading and demarcation"]
[null,null,"a.      Screening for unsightly works","sum",1]
[null,null,"b.     Clear demarcating of the working foot print"]
[null,null,"c.      Barricading of sensitive no go areas"]
[]
[4.7,"9.4 to 9.4.6","Pollution prevention and preservation of environmental resources "]
[4.8,null,"The rate for this item shall include costs for  pollution prevention and preservation of environmental resources","sum",1]
[4.9,null,"a) Cleaning the site of litter and rubble","sum",1]
["4.10",null,"b)Weed control on site","sum",1]
[4.11,null,"C)   Waste bins and receptacles that comply with the waste clauses of the Environmental specification.","sum",1]
[4.12,null,"c)  Appropriate skips for waste separation","sum",1]
[4.13,null,"d)General waste Waste removal","sum",1]
[4.14,null,"e)Hazardous waste Waste removal","sum",1]
[4.15,null,"f)Recycled waste management  Waste removal","sum",1]
[4.16,null,"g) Spillage kits to clean up spillages  ","sum",1]
[4.17,null,"h) Hard impervious surfaces for storage of chemicals","sum",1]
[4.18,null,"i)Bunding facility for hazardous products","sum",1]
[4.19,null,"J)          Labelled containers for decanting of liquids","sum",1]
[{"v":4.2,"d":"4.20"},null,"K) Drip trays for all vehicles staying on site over night","sum",1]
[4.21,9.5,"Preservation of the environment: fauna ,flora, scenic value,  Archaeological artefacts"]
[4.21,"9.5.3","Erosion control and silt management The amount shall represent the costs associated with the practice of preventing or controlling wind or water erosion during construction. The erosion control measures must effectively prevent water pollution, soil loss, wildlife habitat loss and human property loss.  The rate shall also include the costs of silt control where devices shall be designed to keep eroded soil on a construction site, so that it does not wash off and cause water pollution to a nearby stream, river, lake, or dam.","Lump Sum",1]
[4.22,null,"Final clean up and rehabilitation of the construction camp to the state in which it was prior to comencement of work","Lump Sum",1]
[4.23,null,"Appointment of an environmental officer fot the duration of the work","sum",1]
[]
[null,null,"Total amount carried forward"]
[]
["SECTION 4: SUMMARY "]
["No","Payment refers","Description",{"$nulls":3},"Amount"]
[null,null,"ENVIRONMENT"]
[]
[]
["Section 4 :  Carried Forward to Summary"]

{"sheet":"4B Quality","index":4,"n_rows":50,"n_cols":7,"rows_kept":50,"merged":[[1,9,1,11],[49,0,49,5]],"flags":["formulas_cached_only"]}
[null,null,"Lethabo Pump Station: ",{"$nulls":3},"Section 4B:  P&G Time Related"]
[null,null,"Header upgrade at Lethabo Pumping Station"]
[]
["Item ","Payment","Description","Unit","Qty","Rate","Amount"]
["No.","Refers"]
[null,"PSA 8.3.14","SECTION 4B : Quality Control and Assurance "]
[]
["4B.1",null,"Preparation and submission of Contractors Quality Management Plan (CQMP), for review and approval prior to commencement of works","  Lump sum",1]
[]
["4B.2",null,"Implementing activities of the Quality Control Plan or Inspection Test Plan activities not specified in the BOQ but included in the QCP/ITP ","  Lump sum",1]
[]
["4B.3",null,"Provision of Qualified Quality Officer ( The contractor shall provide RW with relevant to the scope of work  qualified Quality Officer )","Lump sum ",1]
[]
["4B.4",null,"Maintenance of documents and final documentation for submission ","Lump sum "]
[]
["4B.5",null,"Provision of Quality Officers relevant training ( The contractor to provide related training for the quality officer ) ",1,1]
[]
["4B.6",null,"Provision of Compliance Audits",1,1]
[]
["4B.7",null,"Testing Equipment calibration Certificates  ( The testing Equipments should be calibrated as per the manual ) ",1,1]
[]
["4B.8",null,"Welders qualification  training as per the code ( The contractors must qualify the welders as per API 5L ) ",1,1]
[]
["4B.9",null,"Provision of any other  testing and inspections requested and appoved  by the Engineer","Lump sum ",1]
[]
["4B.10",null,"Provision of non-destructive tests-"]
[null,"a)","Magnetic Particle Test","Lump sum ",1]
[]
[]
[null,"b)","Radiographic Tests (X-Rays)","Lump sum ",1]
[]
[null,"c)","Ultrasonic Test","Lump sum ",1]
[]
[null,"d)","Guided Ultrasonic Test ","Lump sum ",1]
{"$rows_empty":15}
["Section 4B  :  Carried Forward to Summary"]

{"sheet":"5. Dayworks","index":5,"n_rows":118,"n_cols":13,"rows_kept":118,"merged":[[1,9,1,11],[2,9,2,11],[3,9,3,11],[61,0,61,2],[63,0,63,5],[70,0,70,2],[72,0,72,5],[117,0,118,5],[117,6,118,6]],"flags":["formulas_cached_only"]}
[{"$nulls":6},"Section 5: Dayworks"]
[null,null,"Lethabo Pump Station: ",{"$nulls":6},"No Rates or with rates",null,null,0]
[null,null,"Header upgrade at Lethabo Pumping Station"]
[]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No","Refers"]
[]
[null,null,"SECTION 5: DAYWORKS"]
[]
[null,null,"Allow for dayworks for sundry items not covered by measured items:"]
[]
[5.1,8.7,"LABOUR"]
[]
["5.1.1",null,"Unskilled Labourers","hrs",125]
[{"$nulls":9},0]
["5.1.2",null,"Semi Skilled Labourers","hrs",50]
[]
[5.2,8.7,"LABOUR BY TRADE"]
[]
["5.2.1",null,"Construction Hand and Operator","hrs",50]
[]
["5.2.2",null,"Carpenter","hrs",15]
[]
["5.2.3",null,"Clerk","hrs",15]
[]
["5.2.4",null,"Artisans","hrs",25]
[]
["5.2.5",null,"Foreman","hrs",25]
[]
["5.2.6",null,"Gangers and Section Leaders","hrs",25]
[]
["5.2.7",null,"Steel fixer","hrs",12]
[]
["5.2.8",null,"Bricklayer or Plasterer","hrs",12]
[]
["5.2.9",null,"Welder","hrs",12]
[]
[5.3,8.7,"MATERIALS"]
[]
["5.3.1",null,"Provisional sum for cost of material","Prov.Sum",1,{"v":150000,"d":"150,000"},{"v":150000,"d":"150,000"}]
[]
["5.3.2",null,"Contractors mark-up on material","%",{"v":150000,"d":"150,000"}]
[]
[5.4,8.7,"PLANT"]
[]
[null,null,"Tenderers to insert the hire rate at which each item will be charged, which is to cover all relevant costs of plant hire, including operating crew"]
[]
["5.4.1",null,"Lowbed transport of plant to and from site","t.km",500]
[]
["5.4.2",null,"Bulldozer and ripper (D6 or equivalent)","hrs",10]
[]
["5.4.3",null,"Grader (120G or equivalent)","hrs",10]
[]
["5.4.4",null,"Front end wheel loaders (Cat 950 or similar)","hrs",10]
[]
["5.4.5",null,"Back acting excavators (Hitachi EX200 or similar)","hrs",10]
[]
["5.4.6",null,"T L B","hrs",10]
[]
["5.4.7",null,"Tractors and drawn trailers and rollers","hrs",10]
[]
["Total brought forward "]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate","Amount"]
["Total Carried Forward  "]
[]
["5.4.8",null,"Compactors (D72Y or equivalent)","hrs",10]
[]
[]
[]
[]
["Total brought forward "]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate","Amount"]
["Total Carried Forward  "]
[]
["5.4.9",null,"Compressors (250CFM or equivalent)","hrs",20]
[]
["5.4.10",null,"Trucks (7t or equivalent)","hrs",20]
[]
["5.4.11",null,"Tip Trucks (10t or equivalent)","hrs",20]
[]
["5.4.12",null,"Water Tanker","hrs",20]
[]
["5.4.13",null,"Plate Compactor","hrs",20]
[]
["5.4.14",null,"Light delivery vehicles (1t or equivalent)","km",1500]
[]
["5.4.15",null,"Site Boom","No.",20]
[]
["5.4.16",null,"Generator","No.",20]
{"$rows_empty":28}
["Section 5 :  Carried Forward to Summary"]

{"sheet":"6. Civil - Site Clearance","index":6,"n_rows":57,"n_cols":7,"rows_kept":57,"merged":[[6,1,7,1]],"flags":["formulas_cached_only"]}
[null,null,"Lethabo Pump Station: ",{"$nulls":3},"SANS 1200C"]
[null,null,"Header upgrade at Lethabo Pumping Station",{"$nulls":3},"Site Clearance"]
[]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No","Refers"]
[]
["6","SANS 1200C","SECTION 6:  SITE CLEARANCE FOR CHAMBERS"]
[]
[]
["6.1","8.2.1","Clear and grub","ha",{"v":0.49,"d":"0.490"}]
[]
["6.2","8.2.4","Reclear surfaces (only on instructions from the engineer)","ha",0.245]
[]
["6.3","8.2.8","Demolish and remove existing valve chambers/structures and dismatle steelwork within Lethabo pumping station (refer to dwg. R09160/002) as well as along the B5 and B11 pipelines located outside the station (refer to dwg. no.: R09160/018). This rate shall cover the cost of demolishing, protection of services, loading, transporting and dumping of the rubble and any charges for the use of a dumping site"]
[]
["6.3.1",null,"a) Water Hammer Tank Foundation (14m x 14m)","Sum ",1]
["6.3.2",null,"b) 2 No. Off Water Hammer Tank Valve Chambers (6m x 5m x 8m high)","Sum ",1]
["6.3.3",null,"c) 2 No. Off (4m x 4m x 8m high)","Sum ",1]
["6.3.4",null,"d) 1 No. Off (6.5m x 4m x 8m high)","Sum ",1]
["6.3.5",null,"e) 1 No. Off (7.5m x 5m x 8m high)","Sum ",1]
["6.3.6",null,"f) 1 No. Off (5m x 6m x 8m high)","Sum ",1]
["6.3.7",null,"g) 1 No. Off (3m x 3m x 6m high)","Sum ",1]
["6.3.8",null,"h) 1 No. Off (5m x 6m x 6m high)","Sum ",1]
["6.3.9",null,"i) 4 No. Off (3m x 3m x 7m high)","Sum ",1]
["6.3.10",null,"j) 1 No. Off (6m x 5m x 6m high)","Sum ",1]
["6.3.11",null,"k) B5 and B11 existing Air valve chambers outside Lethabo pump station","Sum ",1]
[]
["6.4","8.2.10","Remove topsoil to nominal depth of 150mm and stockpile","m3",310]
{"$rows_empty":28}
[null,null,"Section 6 :Carried Forward to Summary",{"$nulls":3},0]

{"sheet":"7. Civil - Earthworks","index":7,"n_rows":52,"n_cols":7,"rows_kept":52,"merged":[[6,1,7,1]],"flags":["formulas_cached_only"]}
[null,null,"Lethabo Pump Station: ",{"$nulls":3},"SANS 1200DA"]
[null,null,"Header upgrade at Lethabo Pumping Station",{"$nulls":3},"Earthworks (Small Works)"]
[]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No","Refers"]
[]
[7,"SANS 1200DA","SECTION 7:  EARTHWORKS FOR CHAMBERS"]
[]
[]
[7.1,"8.3.1(b)","Excavate in all materials and  dispose as ordered. All haul for this contract shall be regarded as freehaul.  The cost of transportation of all materials will be deemed to be included in the rates and prices tendered.","m3",2730]
[]
[7.2,"8.3.1 (c)","Extra-over for:"]
[null,null,"1) hard rock excavation (Provisional)","m3",273]
[]
[7.43,"8.3.4","Importing of  material from a commercial source"]
[]
["7.3.1","8.3.4.1","Importing of backfill G7 Material compacted in layers not exceeding 150mm in thickness compacted to 93% MOD AASHTO density AT -1% to +2% OMC","m3",14309]
[]
["7.3.2",null,"Extra over for 8.3.1(b)","m3",{"v":1430.9,"d":"1431"}]
[]
["7.3.3","8.3.4.2","G5 Material compacted in layers not exceeding 100 mm in thickness compacted to 95% MOD AASHTO density AT -1% to +2% OMC","m3",715]
[]
[7.4,"8.3.6","Topsoiling from stockpile and planting of grass ","m2",1012]
[]
[7.5,"8.3.7","Planting of grass from commercial sources to match what is on site","m2",1012]
[]
[7.6,"8.3.8","Traffic signs","Sum",1]
[]
[]
[]
[]
[]
[null,null,"NOTE:"]
[null,null,"Classes Of Excavation"]
[]
[null,null,"Under this contract soft and intermediate excavation shall be classified together as soft excavation, and hard rock and boulder excavation, where boulders are larger than 1 m3, shall be classified together as hard rock excavation.  Boulders smaller than 1 m3 shall be classified together with soft excavation. "]
{"$rows_empty":15}
[null,null,"Section  7:  Carried Forward to Summary",{"$nulls":3},0]

{"sheet":"8. Civil - Concrete","index":8,"n_rows":347,"n_cols":7,"rows_kept":347,"merged":[[60,0,60,2],[64,0,64,2],[109,0,109,2],[113,0,113,2],[177,0,177,2],[181,0,181,2],[236,0,236,2],[240,0,240,2],[281,0,281,2],[285,0,285,2]],"flags":["formulas_cached_only"]}
[null,null,"Lethabo Pump Station: ",{"$nulls":3},"SANS 1200GA"]
[null,null,"Header upgrade at Lethabo Pumping Station",{"$nulls":3},"Concrete (Valve chambers)"]
[]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No","Refers"]
[]
[8,"SABS\n1200GA","SECTION 8: CONCRETE (VALVE CHAMBERS)"]
[]
[8.1,"8.2","Formwork"]
[]
["8.1.1","8.2.1","Rough formwork (sides of base slab)","m²",346]
[]
["8.1.2","8.2.2","Smooth formwork","m²",4577]
[]
["8.1.3","8.2.3","Narrow widths"]
[]
["8.1.3.1",null,"Sides of roof slab (230mm high)","m",315]
[]
["8.1.3.2",null,"Sides of roof panels (150-180mm high)","m",865]
[]
["8.1.3.3",null,"Sides of roof panels (200-230mm high)","m",105]
[]
["8.1.3.4",null,"Sides of base slab (600mm high)","m",82]
[]
["8.1.3.5",null,"Sides of base slab (550mm high)","m",140]
[]
["8.1.3.6",null,"Sides of base slab (500mm high)","m",160]
[]
["8.1.3.7",null,"Side of NRV valve plinths (500mm)","m",40]
[]
["8.1.3.8",null,"To form sides of sump below floor (200mm high)","m",28]
[]
["8.1.3.9",null,"Sides of upstand beams (200mm high)","m",270]
[]
["8.1.4","8.2.4","Box out Holes / Form Voids"]
[]
["8.1.4.1",null,"Chamber 2A - box out hole for 1.8m diameter pipe for depth 500mm thick wall","No.",2]
[]
["8.1.4.2",null,"Chamber 2A - box out hole for 0.4m diameter pipe for depth 500mm thick wall","No.",1]
[]
["8.1.4.3",null,"Chamber 2A - box out hole for 0.25m diameter pipe for depth 230mm thick removable roof panel","No.",1]
[]
["8.1.4.4",null,"Chamber 2B - box out hole for 1.8m diameter pipe for depth 500mm thick wall","No.",2]
[]
["8.1.4.5",null,"Chamber 2B - box out hole for 0.4m diameter pipe for depth 500mm thick wall","No.",1]
[]
["8.1.4.6",null,"Chamber 2B - box out hole for 0.25m diameter pipe for depth 230mm thick removable roof panel","No.",1]
[]
["8.1.4.7",null,"Chamber 3 - box out hole for 2.0m diameter pipe for depth 450mm thick wall","No.",2]
[]
["8.1.4.8",null,"Chamber 3 - box out hole for 0.25m diameter pipe for depth 180mm thick removable roof panel","No.",1]
[]
["8.1.4.9",null,"Chamber 4 - box out hole for 2.0m diameter pipe for depth 400mm thick wall","No.",2]
[]
["8.1.4.10",null,"Chamber 4 - box out hole for 0.25m diameter pipe for depth 180mm thick removable roof panel","No.",1]
[]
[]
[]
[]
[]
["Total Carried Forward ",{"$nulls":5},0]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No","Refers"]
[]
["Total brought forward "]
[]
["8.1.4.11",null,"Chamber 5 - box out hole for 1.8m diameter pipe for depth 400mm thick wall","No.",2]
[]
["8.1.4.12",null,"Chamber 5 - box out hole for 0.25m diameter pipe for depth 180mm thick removable roof panel","No.",1]
[]
["8.1.4.13",null,"Chamber 6 - box out hole for 1.8m diameter pipe for depth 400mm thick wall","No.",2]
[]
["8.1.4.14",null,"Chamber 6 - box out hole for 0.25m diameter pipe for depth 180mm thick removable roof panel","No.",1]
[]
["8.1.4.15",null,"Chamber 7 - box out hole for 1.8m diameter pipe for depth 400mm thick wall","No.",2]
[]
["8.1.4.16",null,"Chamber 7 - box out hole for 0.25m diameter pipe for depth 180mm thick removable roof panel","No.",1]
[]
["8.1.4.17",null,"Chamber 8 - box out hole for 1.8m diameter pipe for depth 450mm thick wall","No.",2]
[]
["8.1.4.18",null,"Chamber 8 - box out hole for 1.4m diameter pipe for depth 450mm thick wall","No.",2]
[]
["8.1.4.19",null,"Chamber 8 - box out hole for 0.25m diameter pipe for depth 180mm thick removable roof panel","No.",1]
[]
["8.1.4.20",null,"Chamber 9 - box out hole for 2.5m diameter pipe for depth 450mm thick wall","No.",2]
[]
["8.1.2.21",null,"Chamber 11 - box out hole for 1.8m diameter pipe for depth 500mm thick wall","No.",2]
[]
["8.1.2.22",null,"Chamber 12 - box out hole for 1.8m diameter pipe for depth 450mm thick wall","No.",1]
[]
["8.1.2.23",null,"Chamber 12 - box out hole for 1.4m diameter pipe for depth 450mm thick wall","No.",1]
[]
["8.1.2.23",null,"Chamber 12 - box out hole for 0.25m diameter pipe for depth 180mm thick removable roof panel","No.",1]
[]
["8.1.2.24",null,"Chamber 13 - box out hole for 2.0m diameter pipe for depth 450mm thick wall","No.",2]
[]
["8.1.2.25",null,"Chamber 13 - box out hole for 0.25m diameter pipe for depth 180mm thick removable roof panel","No.",1]
[]
["8.1.2.26",null,"Chamber 13 - box out hole for 0.2m diameter pipe for depth 450mm thick wall","No.",1]
[]
["8.1.2.27",null,"Chamber 14 - box out hole for 1.8m diameter pipe for depth 450mm thick wall","No.",1]
[]
["8.1.2.28",null,"Chamber 14 - box out hole for 1.4m diameter pipe for depth 450mm thick wall","No.",1]
[]
["8.1.2.29",null,"Chamber 14 - box out hole for 0.25m diameter pipe for depth 180mm thick removable roof panel","No.",1]
[]
["8.1.2.30",null,"Chamber 15 - box out hole for 1.8m diameter pipe for depth 450mm thick wall","No.",2]
[]
[]
["Total Carried Forward ",{"$nulls":5},0]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No","Refers"]
[]
["Total brought forward "]
[]
["8.1.2.31",null,"Box out for 500mm x 500mm x 200mm deep sump","No.",14]
[]
[8.2,"8.3","Reinforcement"]
[]
["8.2.1","8.3.1","Steel bars"]
[]
["8.2.1.1",null,"Mild steel reinforcement"]
[]
[null,null,"a) Chamber 2A (excluding base slab)","t",{"v":8.549999999999999,"d":"9"}]
[null,null,"b) Chamber 2B (excluding base slab)","t",{"v":6.8999999999999995,"d":"7"}]
[null,null,"c) Chamber 3","t",{"v":3.9,"d":"4"}]
[null,null,"d) Chamber 4","t",{"v":2.6999999999999997,"d":"3"}]
[null,null,"e) Chamber 5","t",{"v":2.4,"d":"2"}]
[null,null,"f) Chamber 6","t",{"v":2.4,"d":"2"}]
[null,null,"g) Chamber 7","t",{"v":2.1,"d":"2"}]
[null,null,"h) Chamber 8","t",6]
[null,null,"i) Chamber 9","t",{"v":4.05,"d":"4"}]
[null,null,"j) Chamber 11 (excluding base slab)","t",{"v":2.4,"d":"2"}]
[null,null,"k) Chamber 12","t",{"v":6.8999999999999995,"d":"7"}]
[null,null,"l) Chamber 13","t",{"v":3.9,"d":"4"}]
[null,null,"m) Chamber 14","t",{"v":6.8999999999999995,"d":"7"}]
[null,null,"n) Chamber 15","t",{"v":3.3,"d":"3"}]
[null,null,"o) Precast Air Valve chambers","t",{"v":4.8,"d":"5"}]
[null,null,"p) Chamber 2A, 2B, 11 base slab","t",{"v":6.8999999999999995,"d":"7"}]
[]
["8.2.1.2",null,"High tensile steel reinforcement"]
[]
[null,null,"a) Chamber 2A (excluding base slab)","t",57]
[null,null,"b) Chamber 2B (excluding base slab)","t",46]
[null,null,"c) Chamber 3","t",26]
[null,null,"d) Chamber 4","t",18]
[null,null,"e) Chamber 5","t",16]
[null,null,"f) Chamber 6","t",16]
[null,null,"g) Chamber 7","t",14]
[null,null,"h) Chamber 8","t",40]
[null,null,"i) Chamber 9","t",27]
[null,null,"j) Chamber 11 (excluding base slab)","t",16]
[null,null,"k) Chamber 12","t",46]
[null,null,"l) Chamber 13","t",26]
[null,null,"m) Chamber 14","t",46]
[null,null,"n) Chamber 15","t",22]
[null,null,"o) Precast Air Valve chambers","t",32]
[null,null,"p) Chamber 2A, 2B, 11 base slab","t",46]
[]
["8.2.1.3","8.3.2","High-tensile welded mesh Ref. 395 including mesh stools"]
[]
[null,null,"a) Precast Air Valve Chamber (Dwg. R09160/018)","m2",937]
[]
[8.3,"8.4","Concrete"]
[]
["8.3.1","8.4.2","75mm thick Class 15/19MPa Blinding Layer:"]
[]
[null,null,"a) Chamber 2A","m2",134]
[null,null,"b) Chamber 2B","m2",114]
[null,null,"c) Chamber 3","m2",2]
[null,null,"d) Chamber 4","m2",43]
[null,null,"e) Chamber 5","m2",37]
[null,null,"f) Chamber 6","m2",34]
[null,null,"g) Chamber 7","m2",34]
[null,null,"h) Chamber 8","m2",110]
[]
[]
["Total Carried Forward ",{"$nulls":5},0]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No","Refers"]
[]
["Total brought forward "]
[]
[null,null,"i) Chamber 9","m2",67]
[null,null,"j) Chamber 11","m2",25]
[null,null,"k) Chamber 12","m2",110]
[null,null,"l) Chamber 13","m2",57]
[null,null,"m) Chamber 14","m2",110]
[null,null,"n) Chamber 15","m2",57]
[null,null,"o) Precast Air Valve chambers","m2",469]
[]
["8.3.2","8.4.3","Grade 35MPa/19mm + Xypex Admix C-500NF added to concrete at a dosage of 4 kg/m3:"]
[]
[null,null,"a) Chamber 2A (excluding base slab)","m3",{"v":203.56030995059226,"d":"204"}]
[null,null,"b) Chamber 2B (excluding base slab)","m3",163]
[null,null,"c) Chamber 3","m3",{"v":91.0965666117692,"d":"91"}]
[null,null,"d) Chamber 4","m3",{"v":61.082725877128155,"d":"61"}]
[null,null,"e) Chamber 5","m3",{"v":54.10744796047381,"d":"54"}]
[null,null,"f) Chamber 6","m3",{"v":56.99987614034052,"d":"57"}]
[null,null,"g) Chamber 7","m3",{"v":48.167876140340525,"d":"48"}]
[null,null,"h) Chamber 8","m3",{"v":140.90894263153234,"d":"141"}]
[null,null,"i) Chamber 9","m3",{"v":94.56463533088939,"d":"95"}]
[null,null,"j) Chamber 11 (excluding base slab)","m3",54]
[null,null,"k) Chamber 12","m3",{"v":162.44144263153237,"d":"162"}]
[null,null,"l) Chamber 13","m3",{"v":91.0965666117692,"d":"91"}]
[null,null,"m) Chamber 14","m3",{"v":162.44144263153237,"d":"162"}]
[null,null,"n) Chamber 15","m3",{"v":75.86944796047379,"d":"76"}]
[null,null,"o) Precast Air Valve chambers","m3",{"v":114.10199999999995,"d":"114"}]
[null,null,"p) Chamber 2A, 2B, 11 base slab","m3",163]
[]
["8.3.3","8.4.3","Grade 5MPa:"]
[]
[null,null,"External mass concrete access steps (Refer to Dwg: RA27329)","m3",16]
[]
[8.4,"8.4.4","Unformed surface finishes"]
[]
["8.4.1",null,"Wood-floated finish to floor and roof slabs","m2",2385]
[]
[8.5,"8.8","Miscellaneous"]
[]
["8.5.1",null,"Cast in PVC sleeves:"]
[]
["8.5.1.1",null,"100mm diameter (I.D) x 400mm long in wall for sump pump pipe (sealed by Mech. Contractor)","No.",5]
[]
["8.5.1.2",null,"100mm diameter (I.D) x 450mm long in wall for sump pump pipe (sealed by Mech. Contractor)","No.",6]
[]
["8.5.1.3",null,"100mm diameter (I.D) x 500mm long in wall for sump pump pipe (sealed by Mech. Contractor)","No.",3]
[]
["8.5.1.4",null,"110mm diameter x 400mm long including Vermin proof mesh in walls for ventilation","No.",16]
[]
["8.5.1.5",null,"110mm diameter x 450mm long including Vermin proof mesh in walls for ventilation","No.",36]
[]
["8.5.1.6",null,"110mm diameter x 500mm long including Vermin proof mesh in walls for ventilation","No.",18]
[]
[]
[]
["Total Carried Forward ",{"$nulls":5},0]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No","Refers"]
[]
["Total brought forward "]
[]
["8.5.1.7",null,"110mm diameter x 400mm long in walls (sealed by Elec. Contractor)","No.",15]
[]
["8.5.1.8",null,"110mm diameter x 450mm long in walls (sealed by Elec. Contractor)","No.",18]
[]
["8.5.1.9",null,"110mm diameter x 500mm long in walls (sealed by Elec. Contractor)","No.",9]
[]
["8.5.1.10",null,"250mm diameter x 230mm long  (for actuator shaft)","No.",2]
[]
["8.5.1.11",null,"250mm diameter x 180mm long  (for actuator shaft)","No.",11]
[]
["8.5.1.12",null,"50mm diameter x 150mm long in walls with Vermin proof mesh inside and out (Precast Air Valve Chamber walls  Dwg.: RA9160/003) ","No.",168]
[]
["8.5.1.13",null,"50mm diameter x 150mm long for lifting purposes (Precast chamber roof to be capped and sealed)","No.",168]
[]
["8.5.1.14",null,"30mm diameter (I.D) x 180mm long in roof panels for guide pin","No.",228]
[]
["8.5.1.15",null,"30mm diameter (I.D) x 230mm long in roof panels for guide pin","No.",14]
[]
["8.5.2",null,"Supply and cast in standard Rand Water frame and sump cover (Dwg.: A8879)","No.",14]
[]
["8.5.3",null,"Cast in standard Rand Water manhole frame and cover (supplied by Rand Water; Dwg.: 11860))","No.",58]
[]
["8.5.4",null,"Supply and install standard Rand Water grab rail (Dwg.: A9858)","No.",58]
[]
["8.5.5",null,"Supply and install 12mm diameter holding down bolts (see details on Drg. No. RA26809/5)","No.",44]
[]
["8.5.6",null,"Gundle brickgrip  DPC 375 bond breaker or similar approved for removable roof panels","m2",180]
[]
["8.5.7",null,"Rigid polymer modified liquid waterproofing ( Refer to Concrete Note: 10 on General Arrangement Drawings of Valve Chambers)","m2",4850]
[]
["8.5.8",null,"Supply in install fast curing, one component polyurethane sealant and adhesive 'SIKA SIKAFLEX-11FC + I-CURE or similar approved along all roof panel joints and openings for dowels (excl. precast chambers)","m",420]
[]
["8.5.9",null,"Guide Pin: Supply and install 20mm O.D. steel bar (390mm long) doweled 200mm into top of wall together with an approved reinforcement fixing epoxy","No.",14]
[]
["8.5.10",null,"Guide Pin: Supply and install 20mm O.D. steel bar (340mm long) doweled 200mm into top of wall together with an approved reinforcement fixing epoxy","No.",228]
[]
[]
[]
[]
["Total Carried Forward ",{"$nulls":5},0]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No","Refers"]
[]
["Total brought forward "]
[]
["8.5.11",null,"Galvanized Y16 reinforcing bar in removable roof panels (Refer to detail on the General arrangement drawings)","No.",242]
[]
["8.5.12",null,"Hoisting and putting into place removable roof panels","No.",121]
[]
["8.5.13",null,"Steel valve supports with shims (refer to Dwg. Nos.: R09160/200 - R09160/217 and RW Standard Dwg.: A12210)","No.",32]
[]
["8.5.14",null,"Rip and re-compact the base of the excavation to 93% MOD AASHTO density at -1% to +2% of optimum moisutre content","m2",1403]
{"$rows_empty":52}
[null,null,"Section 8 :  Carried Forward to Summary",{"$nulls":3},0]

{"sheet":"9. Civil - Precast Concrete","index":9,"n_rows":107,"n_cols":7,"rows_kept":107,"merged":[[39,0,39,2],[43,0,43,2]],"flags":["formulas_cached_only"]}
[null,null,"Lethabo Pump Station: ",{"$nulls":3},"SANS 1200GE"]
[null,null,"Header upgrade at Lethabo Pumping Station",{"$nulls":3},"Precast Concrete (Structural)"]
[]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No","Refers"]
[]
[9,"SABS\n1200GE","SECTION 9: PRECAST CONCRETE (STRUCTURAL) - Air Valve Chambers"]
[]
[9.1,"8.2.1","Provide Structural Precast Units"]
[null,null,"(The Qty. indicated below is for a complete Air Valve Chamber. Refer to Dwg.: R09160/018 and R09160/019)"]
[]
["9.1.1",null,"a) Provide 2800x3300x500mm high Precast Concrete Chamber units for a 5m high chamber with a 150mm wall thickness","No.",2]
[]
["9.1.2",null,"b) Provide 2800x3300x500mm high Precast Concrete Chamber units for a 4.5m high chamber with a 150mm wall thickness","No.",13]
[]
["9.1.3",null,"c) Provide 2800x3300x500mm high Precast Concrete Chamber units for a 4m high chamber with a 150mm wall thickness","No.",22]
[]
["9.1.4",null,"d) Provide 2800x3300x500mm high Precast Concrete Chamber units for a 3.5m high chamber with a 150mm wall thickness","No.",2]
[]
["9.1.5",null,"e) Provide 2800x3300x500mm high Precast Concrete Chamber units for a 3m high chamber with a 150mm wall thickness","No.",2]
[]
["9.1.6",null,"f) Provide 2800x3300x500mm high Precast Concrete Chamber units for a 2.5m high chamber with a 150mm wall thickness","No.",2]
[]
["9.1.7",null,"g) Provide 2800x3300x150mm thick Precast Concrete Roof Slab","No.",43]
[]
[9.2,"8.2.2","Erection of Structural Precast Units"]
[null,null,"(the rate is inclusive of all joint sealing systems, waterproof membranes, motar seals, bandages, grouting, sealants, adhesives, staggered step irons etc. as per Dwg.: R09160/018 and R09160/019)"]
[]
["9.2.1",null,"a) Erect 2800x3300x500mm high Precast Concrete Chamber units for a 5m high chamber with a 150mm wall thickness","No.",2]
[]
["9.2.2",null,"b) Provide 2800x3300x500mm high Precast Concrete Chamber units for a 4.5m high chamber with a 150mm wall thickness","No.",13]
[]
["9.2.3",null,"c) Provide 2800x3300x500mm high Precast Concrete Chamber units for a 4m high chamber with a 150mm wall thickness","No.",22]
[]
["9.2.4",null,"d) Provide 2800x3300x500mm high Precast Concrete Chamber units for a 3.5m high chamber with a 150mm wall thickness","No.",2]
[]
["9.2.5",null,"e) Provide 2800x3300x500mm high Precast Concrete Chamber units for a 3m high chamber with a 150mm wall thickness","No.",2]
[]
[]
["Total Carried Forward "]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No","Refers"]
[]
["Total brought forward "]
[]
["9.2.6",null,"f) Provide 2800x3300x500mm high Precast Concrete Chamber units for a 2.5m high chamber with a 150mm wall thickness","No.",2]
[]
["9.2.7",null,"g) Provide 2800x3300x150mm thick Precast Concrete Roof Slab","No.",43]
[]
[9.3,null,"Supply and install precast scour chamber including the cast in-situ floor slab as per drawing - Refer to drwaing number RA28061. Rate to include supply and installation of water proofing membrane to the walls of the the dry well, refer to R09160/018 for details.","No.",1]
{"$rows_empty":56}
[null,null,"Section 9 :  Carried Forward to Summary",{"$nulls":3},0]

{"sheet":"10. Civil - Structural Steel","index":10,"n_rows":55,"n_cols":7,"rows_kept":55,"flags":["formulas_cached_only"]}
[null,null,"Lethabo Pump Station: ",{"$nulls":3},"SANS 1200HA"]
[null,null,"Header upgrade at Lethabo Pumping Station",{"$nulls":3},"Structural steelwork (Sundry items)"]
[]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No","Refers"]
[]
[10,"SABS\n1200HA","SECTION 10: STRUCTURAL STEELWORK (SUNDRY ITEMS)"]
[]
[null,"8.3","Scheduled Items"]
[]
[10.1,"8.3.3","Ladders complete and installed"]
[]
["10.1.1",null,"a) Supply and install standard Rand Water internal catladders (for cat ladder lengths refer to drawings R09160/200 - R09160/219; R09160/400; R09160/402)\n","Sum",1]
[]
["10.1.2","8.3.1","Structural steel (Supply and install complete steel platforms excluding catladders (see dwg. R09160/400 - R09160/401)","Sum",1]
{"$rows_empty":39}
[null,null,"Section 10  Carried Forward to Summary",{"$nulls":3},0]

{"sheet":"11. Pipeline - Site Clearance","index":11,"n_rows":71,"n_cols":7,"rows_kept":71,"merged":[[5,10,6,10],[6,1,7,1],[26,1,27,1],[47,1,48,1],[49,1,50,1],[70,0,71,5],[70,6,71,6],[74,1,75,1],[74,9,75,13]],"flags":["formulas_cached_only"]}
[null,null,"Lethabo Pump Station: ",{"$nulls":3},"Section 11: Site Clearance"]
[null,null,"Header upgrade at Lethabo Pumping Station"]
[]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No","Refers"]
[]
[11,"SABS 1200C","SECTION 11:  SITE CLEARANCE"]
[]
[]
[11.1,null,"Site Clearance"]
[]
["11.1.1","8.2.1","Clear and grub vegetation and trees of girth up to 1m  along the route of the mainline  (see PS2.6 & PSC 5.9) ","m",720]
[]
["11.1.2","8.2.2 ","Clear trees of girth and designated obstacles (see PS2.6 & PSC 5.10)"]
[]
["11.1.2.1",null,"a) over 1m and up to and including 2m","No",2]
[]
["11.1.2.2",null,"b) over 2m m and up to and including 3m","No",2]
[]
["11.1.2.3",null,"c) over 3m in steps of 1m","No",5]
[]
[11.2,null,"Remove and stockpile topsoil"]
[]
["11.2.1","8.2.10 ","Remove and stockpile topsoil to a depth of 300mm along the route of the pipeline (within working servitude) and maintain","m2",800]
[]
[]
[11.3,null,"Dealing with existing Fences and Walls"]
[]
["11.3.1","PSC  8.2.11","Removal of fencing, storage during construction and reinstallation once construction is complete"]
[]
["11.3.1.1",null,"Type 1: Barbed wire fencing up to 1.2m high","m",5]
[]
["11.3.1.2",null,"Type 2: Diamond mesh fencing up to 1.2m high","m",20]
[]
["11.3.1.3",null,"Type 3: Razor mesh wire fencing up to 2.4m high","m",20]
[]
[]
[11.4,null,"Crossing existing Fences"]
[]
["11.4.1","PSC\n8.2.12","Install 5m wide x 1.2m high double gate with 20m refurbished fencing","No",1]
[]
[11.5,null,"Fire breaks"]
[]
["11.5.1","PSC 8.2.13","Form fire breaks on Engineer's Instruction","m²",500]
[]
[]
[]
["11.6",null,"Topsoiling"]
[]
["11.6.1","PSDB  8.3.6.2","Place topsoil to a depth of 150mm","m2",{"v":2000,"d":"2,000"}]
[]
[]
["11.7","SANS 1200D","Vegetation Re-establishment"]
[]
["11.7.1","8.3.11","Hydroseeding with appropriate grass seed mix. (Deemed to be inclusive of soil preparation and improvements, materials and labour).","m2",{"v":1000,"d":"1,000"}]
{"$rows_empty":15}
["Section 11 Carried Forward to Summary"]

{"sheet":"12. Pipeline - Earthwork & Bed","index":12,"n_rows":179,"n_cols":7,"rows_kept":179,"merged":[[52,0,52,2],[54,0,54,5],[107,0,107,2],[109,0,109,5],[165,0,165,2],[167,0,167,5],[178,0,179,5],[178,6,179,6]],"flags":["formulas_cached_only"]}
[null,null,"Lethabo Pump Station: "]
[null,null,"Header upgrade at Lethabo Pumping Station",{"$nulls":3},"Section 12:  Earthworks & Bedding"]
[]
["Section 12 : Earthworks & Bedding "]
[null,null,0]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate","Amount"]
[]
[12,null,"SECTION 12:  EARTHWORKS & BEDDING"]
[]
[]
[]
[]
[12.2,"SANS 1200DB","EARTHWORKS (PIPE TRENCHES)"]
[]
[null,null,"Note: Rate to include for forming \"foxholes\" to facilitate welding in the field"]
[]
["12.2.1","8.3.2","Excavation, in all materials for trenches 2.8m wide, backfill, compact and dispose of surplus unsuitable material, for pipes 1800mm nominal diameter for the following depths below.  Rate to include for all temporary works including benching, shoring and dewatering where necessary:"]
[]
[null,null,"      Over                Up to and including"]
[]
["12.2.1.1",null,"a)   1m                   2,0m","m ",5]
[]
["12.2.1.2",null,"b)   2,0m                3,0m","m ",40]
[]
["12.2.1.3",null,"c)   3,0m                4,0m","m ",200]
[]
["12.2.1.4",null,"d)   4,0m                5,0m","m ",60]
[]
["12.2.1.5",null,"e)   5,0m                6,0m","m ",120]
[]
["12.2.1.6",null,"f)    6,0m                7,0m","m ",120]
[]
["12.2.2","8.3.2","Excavation, in all materials for trenches 3.2m wide, backfill, compact and dispose of surplus unsuitable material, for pipes 2000mm nominal diameter for the following depths below.  Rate to include for all temporary works including benching, shoring and dewatering where necessary:"]
[]
[null,null,"      Over                Up to and including"]
[]
["12.2.2.1",null,"a)   0m                   2,0m","m ",0]
[]
["12.2.2.2",null,"b)   2,0m                3,0m","m ",0]
[]
["12.2.2.3",null,"c)   3,0m                4,0m","m ",5]
[]
["12.2.2.4",null,"d)   4,0m                5,0m","m ",5]
[]
["12.2.2.5",null,"e)   5,0m                6,0m","m ",50]
[]
["12.2.2.6",null,"f)    6,0m                7,0m","m ",75]
[]
[]
[]
[]
[]
["Total brought forward "]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate","Amount"]
["Total Carried Forward  "]
[]
["12.2.3",null,"Excavation, in all materials for trenches 1m wide, backfill, compact and dispose of surplus unsuitable material, for pipes 400mm nominal diameter for the following depths below.  Rate to include for all temporary works including benching, shoring and dewatering where necessary:"]
[]
[null,null,"      Over                Up to and including"]
[]
["12.2.3.1",null,"a)   1m                   2,0m","m ",200]
[]
["12.2.3.2",null,"b)   2,0m                3,0m","m ",100]
[]
["12.2.3.3",null,"c)   3,0m                4,0m","m ",3]
[]
["12.2.3.4",null,"d)   4,0m                5,0m","m "]
[]
["12.2.3.5",null,"e)   5,0m                6,0m","m "]
[]
["12.2.3.6",null,"f)    6,0m                7,0m","m "]
[]
[]
["12.2.4","PSDB\n8.3.2(b)(2) ","Extra over Items 7.2.1 to 7.2.5 for excavation in\nhard rock and boulder excavation in excess of 0.5m³","m³",{"v":1000,"d":"1,000"}]
[]
["12.2.5","PSDB 8.3.8","Hand excavation and backfill in soft material to prove existing services to a maximum depth of 2m (Rate to include for all temporary works including benching, shoring and dewatering where necessary):","m³",500]
[]
["12.2.6","PSDB 8.3.8","Hand excavation and backfill in soft material to prove existing services to a maximum depth of 2m (Rate to include for all temporary works including benching, shoring and dewatering where necessary):","m³",0]
[]
["12.2.7","8.3.2(c)","Excavate unsuitable material from trench bottom and dispose","m³",100]
[]
["12.2.8","8.3.3.1","Make up deficiency in backfill material,"]
[]
["12.2.8.1",null,"a)  From other necessary excavations on site","m³",200]
[]
["12.2.8.2",null,"b)  From designated borrow pits","m³",100]
[]
["12.2.8.3",null,"c)  By importation from commercial sources","m³",{"v":4600,"d":"4,600"}]
[]
["12.2.8.4","PSDB 8.3.3.1d","d)  By sieving from excavated materials","m³",10]
[]
[12.3,null,"Unstable trench bottom"]
[]
["12.3.1","PSA 8.10","Supply and install 19 mm crushed stone (Complete as indicated on Drawing RA27141)","m³",50]
[]
["12.3.2","PSDB 8.3.11","Supply and install geotextile filter blanket (Grade A6) (Complete as indicated on Drawing RA27141)","m2",100]
[]
[12.4,null,"Existing services"]
[]
["12.4.1","8.3.5(a)","Existing services that intersect a trench:"]
[]
["12.4.1.1",null,"Stormwater pipes up to 600m diameter","No",0]
[]
["12.4.1.2",null,"Stormwater pipes and culverts larger than 600m diameter","No",0]
[]
["12.4.1.3",null,"Water mains up to 250mm diameter","No",0]
[]
["Total brought forward "]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate","Amount"]
["Total Carried Forward  "]
[]
[]
["12.4.1.4",null,"Water mains larger than 250mm diameter","No",2]
[]
["12.4.1.5",null,"Sewer mains up to 250mm diameter","No",0]
[]
["12.4.1.6",null,"Sewer mains larger than 250mm diameter","No",0]
[]
["12.4.1.7",null,"Underground Electrical Cables (LT and HT)","No",10]
[]
["12.4.1.8","PSDB\n8.3.5(b)","Overhead Electrical Cables","No",0]
[]
["12.4.1.9","PSDB\n8.3.5(c)","Overhead Communication Cables (incl Telkom)","No",0]
[]
["12.4.1.10","PSDB\n8.3.5(d)","Underground Communication Cables (incl Telkom)","No",2]
[]
[]
["12.4.2","8.3.5(a)","Existing Services that adjoin a trench:"]
[]
[null,null,"Note: Price tendered for excavation is to include for working close to existing Rand Water pipelines"]
[]
["12.4.2.1",null,"Stormwater pipes up to 600m diameter","m",0]
[]
["12.4.2.2",null,"Stormwater pipes and culverts larger than 600m diameter","m",0]
[]
["12.4.2.3",null,"Water mains up to 250mm diameter","m",0]
[]
["12.4.2.4",null,"Water mains larger than 250mm diameter","m",100]
[]
[]
[]
[12.5,"SANS 1200LB","BEDDING"]
[]
["12.5.1","PSLB 8.2.1","Provision of bedding from trench excavation of:"]
[]
["12.5.1.1",null,"Selected fill and granular material (stage 1 material as per DRG No RA 27141)","m³",50]
[]
["12.5.2","PSLB 8.2.2.2","Provision of bedding from approved borrow pits including all costs for additional handling and transport."]
[]
["12.5.2.1",null,"Selected fill and granular material (stage 1 material as per DRG No RA 27141)","m³",50]
[]
["12.5.3"," PSLB 8.2.2.3","Provision of bedding from commercial or off site sources of."]
[]
["12.5.3.1",null,"Selected fill and granular material (stage 1 material as per DRG No RA 27141)","m³",{"v":3000,"d":"3,000"}]
[]
["12.5.3.1.1",null,"c)  10mm crushed stone","m³",50]
[]
["12.5.4","8.2.4","Concrete encasement to pipes in Class 20MPa/19mm concrete including reinforcement according to Drawing RA27141 as directed by Engineer (Rate to include for any temporary formwork required).","m³",0]
[]
["12.5.5","PSDB 8.2.2.4.1  ","Soilcrete encasement to pipes according to Drawing RA27141  as directed by the Engineer (Rate to include for any temporary formwork required).","m³",50]
[]
["12.5.6","PSDB 8.2.2.4.2","Cellular lightweight Concrete  encasement to pipes according to Drawing RA27141  as directed by the Engineer (Rate to include for any temporary formwork required).","m³",0]
[]
[]
[]
["Total brought forward "]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate","Amount"]
["Total Carried Forward  "]
[]
[12.6,"SANS 1200DB","FINISHING"]
[]
["12.6.1","8.3.3.3","Compaction of selected fill material for the main fill to 95% Mod AASHTO in areas subjected to loads from road traffic.","m3",3800]
[]
[12.7,null,"Photographic records"]
[]
["12.7.1","PSDA 8.3.10","Take and provide photographic records","Sum",null,{"v":10000,"d":"10,000.00"},{"v":10000,"d":"10,000.00"}]
[]
[]
["Section 12: Carried Forward to Summary"]

{"sheet":"13.Pipeline-Pipes and Specials","index":13,"n_rows":159,"n_cols":7,"rows_kept":159,"merged":[[37,0,37,2],[39,0,39,5],[87,1,88,1],[95,0,95,2],[97,0,97,5],[140,0,140,2],[142,0,142,5],[158,0,159,5],[158,6,159,6]],"flags":["formulas_cached_only"]}
[null,null,"Lethabo Pump Station: ",{"$nulls":3},"Section 13  Steel Pipes & Specials"]
[null,null,"Header upgrade at Lethabo Pumping Station"]
[]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate","Amount"]
[]
[null,null,"SECTION 13: SUPPLY AND INSTALLATION OF"]
[null,null,"STEEL PIPES AND SPECIALS"]
[]
[13.1,"TS1.16.1","Supply and delivery of pipes"]
[]
["13.1.1",null,"Supply and delivery of 400mm ID diameter ASTM A106 Grade B Seamless steel pipe, 9.52mm wall thickness"]
[]
["13.1.1.1",null,"Steel pipe manufacture (m)","m",200]
[]
["13.1.1.2",null,"Internal lining (min 600micron solvent free epoxy lining) as per SANS 1217","m",200]
[]
["13.1.1.3",null,"External coating (Modified Fibre Reinforced Bitumen Material) as per EN 10300:2005 €","m",200]
[]
[13.2,"TS1.16.2","Unload Pipes and specials"]
[]
["13.2.1",null,"Supply and operation of plant and the supply of labour to unload the pipes from the supplier's vehicles and the lay down of the pipes in the temporary lay-down area and/or to certain positions along the route of the pipeline. The cost to supply and/or form storage mounds and measures taken to protect the pipes during this procedure will be included in this item.  This activity will take place on site."]
[]
["13.21.1",null,"2000mm ID diameter Grade B mild steel pipe, 18mm wall thickness","m",70]
[]
["13.2.1.2",null,"1800mm ID diameter Grade B mild steel pipe, 16mm wall thickness","m",450]
[]
["13.2.1.3",null,"400mm ID diameter Grade B mild steel pipe, 9.52mm wall thickness","m",200]
[]
[13.3,"TS1.16.3","Removal / Installation of internal bracing"]
[]
["13.3.1",null,"Supply and operation of plant, supply of material and cost of labour to remove the supplier's internal bracing, return the bracing to the supplier's manufacturing plant, installation of temporary bracing and the removal thereof on completion of backfilling. The cost to repair subsequent damage due to the removal and installation of the bracing will be included in this item.mounds and measures taken to protect the pipes during this procedure will be included in this item.  This activity will take place on site."]
[]
["13.3.1.1",null,"2000mm ID diameter Grade B mild steel pipe, 18mm wall thickness","m",70]
[]
["13.3.1.2",null,"1800mm ID diameter Grade B mild steel pipe, 16mm wall thickness","m",450]
[]
[]
["Total brought forward "]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate","Amount"]
["Total Carried Forward  "]
[13.4,"TS1.16.4","Transporting of pipes and specials to and from lay-down area to side of trench"]
[]
["13.4.1",null,"Supply and operation of plant and cost of labour to load pipes at lay-down area, transport the pipes to the excavated trench or/and point for installation in existing culverts or/and sleeves, regardless of distance and unload the pipes along the trench."]
[]
["13.4.1.1",null,"2000mm ID diameter Grade B mild steel pipe, 18mm wall thickness","Sum",1]
[]
["13.4.1.2",null,"1800mm ID diameter Grade B mild steel pipe, 16mm wall thickness","Sum",1]
[]
["13.4.1.3",null,"400mm ID diameter Grade B mild steel pipe, 9.52mm wall thickness","Sum",1]
[]
[]
[13.5,"TS1.16.5","Install Pipe specials in Trenches"]
[]
["13.5.1",null,"Examine pipes prior to placing in the trench, repair all defects, placing the pipe in the prepared trench including the supply and operation of plant and supply of labour to execute the work, cleaning of joints , Vertical and horizontal lining up of the pipe including the supply and operation of plant and supply of labour to execute the work, supply, installation and removal of protective measures and Internal welding of the joint ."]
[]
["13.5.1.1",null,"2000mm ID diameter Grade B mild steel pipe, 18mm wall thickness","m",70]
[]
["13.5.1.2",null,"1800mm ID diameter Grade B mild steel pipe, 16mm wall thickness","m",450]
[]
["13.5.1.3",null,"400mm ID diameter Grade B mild steel pipe, 9.52mm wall thickness","m",200]
[]
[13.7,"TS1.16.7","External welds"]
[]
["13.7.1",null,"Supply and operation of plant and supply of material and labour to execute the completion of external welds as per as per Clause TS1.6"]
[]
[null,null,"2000mm ID diameter Grade B mild steel pipe, 18mm wall thickness","m",30]
[]
[null,null,"1800mm ID diameter Grade B mild steel pipe, 16mm wall thickness","m",100]
[]
[null,null,"400mm ID diameter Grade B mild steel pipe, 9.52mm wall thickness","m",50]
[]
[8.8,"TS1.16.8","Complete Protective Coating at Joints"]
[]
["8.8.1",null,"Supply and operation of plant and supply of material and cost of labour to execute the completion of internal lining and external coating at the welded joint "]
[]
["13.8.1.1",null,"2000mm ID diameter Grade B mild steel pipe, 18mm wall thickness","No",30]
[]
["13.8.1.2",null,"1800mm ID diameter Grade B mild steel pipe, 16mm wall thickness","No",100]
[]
["13.8.1.3",null,"Flanges for 400mm ID diameter Grade B mild steel pipe, 9.52mm wall thickness using wrapper coating","No",50]
[]
[13.9,"TS1.16.9","Steel Pipe Mitre Bends"]
[]
["13.9.1",null,"Lline-up, cut, clean joints and weld, internally and externally, horizontal and vertical bends and/or mitres over 1° and up to and including 15° cut from pipe supplied by the pipe supplier. Supply and operate plant and supply of material and labour to apply internal lining and external coating to the entire bend and/or mitre as per Clause TS1.7"]
[]
["13.9.1.1",null,"1800mm ID diameter Grade B mild steel pipe, 16mm wall thickness","No",50]
[]
[{"v":13.1,"d":"13.10"},"TS1.16.10","Fabricated Bends"]
[]
[null,null,"Note:  Unless otherwise stated, all steel specials shall be fabricated to BS534 (1990) specifications"]
[]
[null,null,"Supply of complete bends, transport to and unload at point of installation, line-up, install, clean joints and weld, internally and externally, bends over 15° and up to and including 90°.  Supply and operate plant and supply of material and labour to apply internal lining and external coating to the entire bend as per Clause TS1.7"]
[]
["13.10.1",null,"Lobster bends as per DRG No 26732 over 15° up to and including 30° - 2 mitres, 1 full segment."]
[]
["Total brought forward "]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate","Amount"]
["Total Carried Forward  "]
["13.10.1.1",null,"1800mm ID diameter x 16mm wall thickness, Grade B Steel","No",5]
[]
["13.10.2",null,"Lobster bends as per DRG No RA 26732 over 30° up to and including 60° - 2 mitres, 2 full segments."]
[]
["13.10.2.1",null,"1800mm ID diameter x 16mm wall thickness, Grade B Steel","No",1]
[]
[]
[]
[]
[]
["13.10.3",null,"Lobster bends as per DRG No RA 26732 over 60° up to and including 90° - 2 mitres, 3 full segment."]
[]
["13.10.3.1",null,"1800mm ID diameter x 16mm wall thickness, Grade B Steel","No",1]
[]
["13.10.3.2",null,"400mm ID diameter Grade B mild steel pipe, 9.52mm wall thickness","No",20]
[]
[13.11,"TS1.16.15","RADIOGRAPHIC EXAMINATION OF CIRCUMFERENTIAL WELDS"]
[]
["13.11.1",null,"The rate shall cover the cost to appoint a nominated specialist to provide and operate equipment (including mark-up) to execute the radiographic examination of circumferential welds and provide the Engineer with the results and reports of the examinations"]
[]
["13.11.1.1",null,"1800mm and 2000mm diameter pipelines","Sum",1]
[]
[13.12,"TS1 16.16","ACCEPTANCE TESTS"]
[]
["13.12.1",null,"Supply and operate all plant, equipment (including temporary 2:1 steel taper and steel dome welded to pipeline) and machinery and the cost of labour to execute pressure tests as per the requirements of TS1.16 for the pipeline sections and to the test pressure specified by the Engineer."]
[]
["13.12.1.1",null,"1800mm and 2000mm diameter pipelines and tested individually.","Sum",1]
[]
["13.12.1.2",null,"400mm ID diameter Grade B mild steel pipe, 9.52mm wall thickness","Sum",1]
[]
[13.13,"TS1 16.18","CLEANING & DISINFECTION"]
[]
["13.13.1",null,"Supply and operate plant and labour to keep the entire pipes clean  and disinfection of the pipeline after pressure testing in accordance with the Project Specifications as per Clause TS1.13","Sum",1]
[]
[13.14,"TS1.16.19","CHARGING OF PIPELINE"]
[]
["13.14.1",null,"Charging of Pipeline (Water supplied for pipeline hydraulic testing and disinfection by Rand Water) as per Clause TS1.14"]
[]
["13.14.2",null,"1800mm ID diameter Grade B mild steel pipe, 16mm wall thickness","Sum",1]
[]
["13.14.3",null,"2000mm ID diameter Grade B mild steel pipe, 18mm wall thickness","Sum",1]
[]
["Total brought forward "]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate","Amount"]
["Total Carried Forward  "]
[]
[13.15,"TS1.16.22","CUT AND TIE IN TO EXISTING PIPES"]
[]
["13.15.1",null,"Planning of all activities required  prior to shut down of existing pipes. Supply, operate plant and supply of material and labour to cut into existing pipe, cleaning of joints, internal and external welding and repair internal and external coating to the joints as per Clause TS1.9.6"]
[]
["13.15.1.1",null,"Proposed 1800mm diameter steel pipe to tie into existing  2500mm B19 Pipeline.","No",1]
[]
[13.16,null,"CCTV"]
[]
["13.16.1","PSA 8.10 and PS 21","Provide necessary equipment and conduct CCTV for the whole length of the pipe together with bulk water distribution representative prior hand-over.","Sum",1]
[]
["13.16.2",null,"2000mm ID diameter Grade B mild steel pipe, 18mm wall thickness","Sum",1]
[]
["13.16.3",null,"1800mm ID diameter Grade B mild steel pipe, 16mm wall thickness","Sum",1]
[]
["Section 13:  Carried Forward to Summary"]

{"sheet":"14.Pipelines-PipeSpecials M & V","index":14,"n_rows":1096,"n_cols":7,"rows_kept":1096,"merged":[[40,0,40,2],[42,0,42,5],[84,0,84,5],[86,0,86,5],[123,0,123,5],[125,0,125,5],[158,0,158,5],[160,0,160,5],[200,0,200,5],[202,0,202,5],[242,0,242,5],[244,0,244,5],[284,0,284,5],[286,0,286,5],[324,0,324,5],[326,0,326,5],[361,0,361,5],[363,0,363,5],[404,0,404,5],[406,0,406,5],[441,0,441,5],[443,0,443,5],[482,0,482,5],[484,0,484,5],[520,0,520,5],[522,0,522,5],[558,0,558,5],[560,0,560,5],[598,0,598,5],[600,0,600,5],[638,0,638,5],[640,0,640,5],[677,0,677,5],[679,0,679,5],[721,0,721,5],[723,0,723,5],[761,0,761,5],[763,0,763,5],[802,0,802,5],[804,0,804,5],[839,0,839,5],[841,0,841,5],[886,0,886,5],[888,0,888,5],[929,0,929,5],[931,0,931,5],[973,0,973,5],[975,0,975,5],[1020,0,1020,5],[1022,0,1022,5],[1066,0,1066,5],[1068,0,1068,5],[1095,0,1096,5],[1095,6,1096,6]],"flags":["formulas_cached_only"]}
[null,null,"Lethabo Pump Station: ",{"$nulls":3},"Section 14: Pressure Pipework"]
[null,null,"Header upgrade at Lethabo Pumping Station"]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate","Amount"]
[]
[null,null,"SECTION 14:  GENERAL PIPE SPECIALS FOR METER AND VALVE CHAMBERS"]
[]
[14.1,null,"PHASE 1: PIPE SPECIALS"]
[]
["14.1.1",null,"Manufacture and deliver the following pipe specials as per DRG No R0_9160/011.  The rate to include cutting and welding or jointing with flanges as required and for coating and lining as per specifications.  Flanges according to Rand Water specification (DRG No. A11791)"]
[]
["14.1.1.1",null,"1832mm OD, Straight pipe flanged on one end, 10290mm long, 16mm thick, with puddle flange placed at 1100mm from the flange  (1)","No.",1]
[]
["14.1.1.2",null,"1832mm OD, Straight pipe flanged on one end, 10290mm long, 16mm thick (4)","No.",1]
[]
["14.1.1.3",null,"1832 x 1424mm OD concentric reducer with 300mm extensions on either side, flanged on the 1424mm OD side, 16mm thick (5)","No.",2]
[]
["14.1.1.4",null,"1832mm OD straight pipe, flanged on one end, 1575mm long, 16mm thick (7)","No.",1]
[]
["14.1.1.5",null,"1832mm OD straight pipe, flanged on one end, 2500mm long, 16mm thick with puddle flange placed at 1055mm from flange (9)","No.",1]
[]
["14.1.1.6",null,"2036 x 1832mm OD concentric reducer with 300mm extensions on either side, 18mm thick (10)","No.",1]
[]
["14.1.1.7",null,"2036mm OD straight pipe, 7910mm long with 816mm OD stub, 600mm long with flange and collar plate(see item 9.1.1.8) (11)","No.",1]
[]
["14.1.1.8",null,"6mm thick collar plate with 820mm ID & 1210mm OD (12)","No.",2]
[]
["14.1.1.9",null,"DN300 riser piece, flanged both ends. DN300 and DN800 Flanges (13)","No.",2]
[]
["14.1.1.10",null,"2036mm OD, 18mm thick, 45 degree bend (16)","No.",1]
[]
["14.1.1.11",null,"2036mm OD straight pipe, 4470mm long, 18mm thick (17)","No.",1]
[]
["14.1.1.12",null,"2036mm OD, equal tee, 18mm thick (18)","No.",1]
[]
["14.1.1.13",null,"2036mm OD straight pipe, 2475mm long, 18mm thick (19)","No.",1]
[]
["14.1.1.14",null,"2036mm OD x 1836mm OD un-equal tee, 18mm thick (20)","No.",1]
[]
[]
[]
["Total brought forward "]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate","Amount"]
["Total Carried Forward  "]
["14.1.1.15",null,"1832mm OD x 609.6mm OD concentric reducer with 300mm extensions on either sides, 16mm thick (21)","No.",1]
[]
["14.1.1.16",null,"609.6mm OD dome, 425mm long, 12.7mm thick (22)","No.",1]
[]
["14.1.1.17",null,"2036mm OD straight pipe, flanged on one end, 2800mm long, 18mm thick with puddle flange placed at 1390mm from flange (23)","No.",2]
[]
["14.1.1.18",null,"2036mm OD, 18mm thick, 90 degree bend (25)","No.",1]
[]
["14.1.1.19",null,"2036mm OD straight pipe, 14060mm long, 18mm thick (26)","No.",1]
[]
["14.1.1.20",null,"2036mm OD, 18mm thick, 9 degree bend (27)","No.",2]
[]
["14.1.1.21",null,"2036mm OD straight pipe, 9600mm long with 816mm OD stub, 600mm long with flange and collar plate(see item 9.1.1.8) (28)","No.",1]
[]
["14.1.1.22",null,"2036mm OD straight pipe, 14295mm long, 18mm thick (29)","No.",1]
[]
["14.1.1.23",null,"2036mm OD straight pipe, flanged on one end, 3250mm long, 18mm thick with puddle flange placed at 1390mm from flange (30)","No.",2]
[]
["14.1.1.24",null,"2540mm OD x 2036mm OD reducer with 300mm extensions on either sides, 20mm thick (31)","No.",1]
[]
["14.1.1.25",null,"406.4mm OD straight pipe, 665mm long, 9.52mm thick (85)","No.",1]
[]
["14.1.1.26",null,"406.4mm OD, 9.52mm thick, 90 degree bend (86)","No.",4]
[]
["14.1.1.27",null,"406.4mm OD straight pipe, flanged on one end, 9.52mm thick, 500mm long(87)","No.",1]
[]
["14.1.1.28",null,"406.4mm OD straight pipe, flanged on one end, 9.52mm thick, 1500mm long(90)","No.",1]
[]
["14.1.1.29",null,"406.4mm OD straight pipe, 2000mm long, 9.52mm thick (91)","No.",1]
[]
["14.1.1.30",null,"406.4mm OD straight pipe, 2995mm long, 9.52mm thick (92)","No.",1]
[]
["14.1.1.31",null,"406.4mm OD straight pipe, 5470mm long, 9.52mm thick (93)","No.",1]
[]
["14.1.1.32",null,"406.4mm OD straight pipe, 8505mm long, 9.52mm thick (94)","No.",1]
[]
["14.1.1.33",null,"406.4mm OD, equal tee, 18mm thick (95)","No.",1]
[]
["14.1.1.34",null,"406.4mm OD straight pipe, 17000mm long, 9.52mm thick (96)","No.",1]
[]
["14.1.1.35",null,"406.4mm OD straight pipe, 2360mm long, 9.52mm thick (97)","No.",1]
["Total brought forward "]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate","Amount"]
["Total Carried Forward  "]
["14.1.1.36",null,"406.4mm OD straight pipe, 3000mm long, 9.52mm thick (98)","No.",1]
[]
["14.1.1.37",null,"406.4mm OD straight pipe, 8000mm long, 9.52mm thick (99)","No.",1]
[]
["14.1.1.38",null,"406.4mm OD, 9.52mm thick, 45 degree bend (100)","No.",1]
[]
["14.1.1.39",null,"406.4mm OD straight pipe, 22590mm long, 9.52mm thick (101)","No.",1]
[]
["14.1.2",null,"Installation of Pipe specials"]
[null,null,"Collect and install the following pipe specials as per DRG No R0_9160/011.  The rate to include cutting and welding or jointing with flanges as required and for coating and lining as per specifications.  Flanges according to Rand Water specification (DRG No. A11791)"]
[]
["14.1.2.1",null,"1832mm OD, straight pipe flanged on one end, 10290mm long, 16mm thick, with puddle flange placed at 1100mm from the flange  (1)","No.",1]
[]
["14.1.2.2",null,"1832mm OD, straight pipe flanged on one end, 10290mm long, 16mm thick (4)","No.",1]
[]
["14.1.2.3",null,"1832 x 1424mm OD concentric reducer with 300mm extensions on either side, flanged on the 1424mm OD side, 16mm thick (5)","No.",2]
[]
["14.1.2.4",null,"1832mm OD straight pipe, flanged on one end, 1575mm long, 16mm thick (7)","No.",1]
[]
["14.1.2.5",null,"1832mm OD straight pipe, flanged on one end, 2500mm long, 16mm thick with puddle flange placed at 1055mm from flange (9)","No.",1]
[]
["14.1.2.6",null,"2036 x 1832mm OD concentric reducer with 300mm extensions on either side, 18mm thick (10)","No.",1]
[]
["14.1.2.7",null,"2036mm OD straight pipe, 7910mm long with 816mm OD stub, 600mm long with flange and collar plate(see item 9.1.1.8) (11)","No.",1]
[]
["14.1.2.8",null,"6mm thick collar plate with 820mm ID & 1210mm OD (12)","No.",2]
[]
["14.1.2.9",null,"DN300 riser piece, flanged both ends. DN300 and DN800 Flanges (13)","No.",2]
[]
["14.1.2.10",null,"2036mm OD, 18mm thick, 45 degree bend (16)","No.",1]
[]
["14.1.2.11",null,"2036mm OD straight pipe, 4470mm long, 18mm thick (17)","No.",1]
[]
["14.1.2.12",null,"2036mm OD, equal tee, 18mm thick (18)","No.",1]
[]
[]
["Total brought forward "]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate","Amount"]
["Total Carried Forward  "]
["14.1.2.13",null,"2036mm OD straight pipe, 2475mm long, 18mm thick (19)","No.",1]
[]
["14.1.2.14",null,"2036mm OD x 1836mm OD un-equal tee, 18mm thick (20)","No.",1]
[]
["14.1.2.15",null,"1832mm OD x 609.6mm OD concetric reducer with 300mm extensions on either sides, 16mm thick (21)","No.",1]
[]
["14.1.2.16",null,"609.6mm OD dome, 425mm long, 12.7mm thick (22)","No.",1]
[]
["14.1.2.17",null,"2036mm OD straight pipe, flanged on one end, 2800mm long, 18mm thick with puddle flange placed at 1390mm from flange (23)","No.",2]
[]
["14.1.2.18",null,"2036mm OD, 18mm thick, 90 degree bend (25)","No.",1]
[]
["14.1.2.19",null,"2036mm OD straight pipe, 14060mm long, 18mm thick (26)","No.",1]
[]
["14.1.2.20",null,"2036mm OD, 18mm thick, 9 degree bend (27)","No.",2]
[]
["14.1.2.21",null,"2036mm OD straight pipe, 9600mm long with 816mm OD stub, 600mm long with flange and collar plate(see item 9.1.1.8) (28)","No.",1]
[]
["14.1.2.22",null,"2036mm OD straight pipe, 14295mm long, 18mm thick (29)","No.",1]
[]
["14.1.2.23",null,"2036mm OD straight pipe, flanged on one end, 3250mm long, 18mm thick with puddle flange placed at 1390mm from flange (30)","No.",2]
[]
["14.1.2.24",null,"2540mm OD x 2036mm OD reducer with 300mm extensions on either sides, 20mm thick (31)","No.",1]
[]
["14.1.2.25",null,"406.4mm OD straight pipe, 665mm long, 9.52mm thick (85)","No.",1]
[]
["14.1.2.26",null,"406.4mm OD, 9.52mm thick, 90 degree bend (86)","No.",4]
[]
["14.1.2.27",null,"406.4mm OD straight pipe, flanged on one end, 9.52mm thick, 500mm long(87)","No.",1]
[]
["14.1.2.28",null,"406.4mm OD straight pipe, flanged on one end, 9.52mm thick, 1500mm long(90)","No.",1]
[]
["Total brought forward "]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate","Amount"]
["Total Carried Forward  "]
["14.1.2.29",null,"406.4mm OD straight pipe, 2000mm long, 9.52mm thick (91)","No.",1]
[]
["14.1.2.30",null,"406.4mm OD straight pipe, 2995mm long, 9.52mm thick (92)","No.",1]
[]
["14.1.2.31",null,"406.4mm OD straight pipe, 5470mm long, 9.52mm thick (93)","No.",1]
[]
["14.1.2.32",null,"406.4mm OD straight pipe, 8505mm long, 9.52mm thick (94)","No.",1]
[]
["14.1.2.33",null,"406.4mm OD, equal tee, 18mm thick (95)","No.",1]
[]
["14.1.2.34",null,"406.4mm OD straight pipe, 17000mm long, 9.52mm thick (96)","No.",1]
[]
["14.1.2.35",null,"406.4mm OD straight pipe, 2360mm long, 9.52mm thick (97)","No.",1]
[]
["14.1.2.36",null,"406.4mm OD straight pipe, 3000mm long, 9.52mm thick (98)","No.",1]
[]
["14.1.2.37",null,"406.4mm OD straight pipe, 8000mm long, 9.52mm thick (99)","No.",1]
[]
["14.1.2.38",null,"406.4mm OD, 9.52mm thick, 45 degree bend (100)","No.",1]
[]
["14.1.2.39",null,"406.4mm OD straight pipe, 22590mm long, 9.52mm thick (101)","No.",1]
[]
[]
[14.2,null,"PHASE 2: PIPE SPECIALS"]
[]
["14.2.1",null,"Manufacture and deliver the following pipe specials as per DRG No R0_9160/012.  The rate to include cutting and welding or jointing with flanges as required and for coating and lining as per specifications.  Flanges according to Rand Water specification (DRG No. A11791)"]
[]
["14.2.1.1",null,"1832mm OD, straight pipe flanged on one end, 9520mm long, 16mm thick, with puddle flange placed at 1140mm from the flange (1)","No.",1]
[]
["14.2.1.2",null,"1832mm OD, straight pipe flanged on one end, 4580mm long, 16mm thick (4)","No.",1]
[]
["14.2.1.3",null,"1832 x 1424mm OD concentric reducer with 300mm extensions on either side, and flanged on the 1424mm OD side, 16mm thick (5)","No.",2]
[]
["14.2.1.4",null,"1832mm OD straight pipe, flanged on one end, 1780mm long, 16mm thick (7)","No.",1]
[]
["14.2.1.5",null,"1832mm OD straight pipe, flanged on one end, 2160mm long, 16mm thick with puddle flange placed at 1965mm from flange (9)","No.",1]
[]
["14.2.1.6",null,"1832mm OD straight pipe, 8190mm long, 16mm thick (10)","No.",1]
[]
["Total brought forward "]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate","Amount"]
["Total Carried Forward  "]
["14.2.1.7",null,"1832mm OD, 16mm thick, 45 degree bend (11)","No.",1]
[]
["14.2.1.8",null,"1836mm OD straight pipe, 6000mm long with 718mm ID stub, 600mm long with flange and collar plate(see item 9.1.2.9) (12)","No.",1]
[]
["14.2.1.9",null,"6mm thick collar plate with 718mm ID & 1060mm OD (13)","No.",1]
[]
["14.2.1.10",null,"DN300 riser piece, flanged both ends. DN300 and DN800 Flanges (14)","No.",1]
[]
["14.2.1.11",null,"406.4mm OD straight pipe, 675mm long, 9.52mm thick (17)","No.",1]
[]
["14.2.1.12",null,"406.4mm OD, 9.52mm thick, 90 degree bend (18)","No.",3]
[]
["14.2.1.13",null,"406.4mm OD straight pipe, flanged on one end, 9.52mm thick, 500mm long (19)","No.",1]
[]
["14.2.1.14",null,"406.4mm OD straight pipe, flanged on one end, 9.52mm thick, 1600mm long (22)","No.",1]
[]
["14.2.1.15",null,"406.4mm OD straight pipe, 2995mm long, 9.52mm thick (23)","No.",1]
[]
["14.2.1.16",null,"406.4mm OD straight pipe, 1940mm long, 9.52mm thick (24)","No.",1]
[]
["14.2.1.17",null,"406.4mm OD, equal tee, 18mm thick (25)","No.",1]
[]
[]
["14.2.2",null,"Installation of Pipe specials"]
[null,null,"Collect and install the following pipe specials as per DRG No R0_9160/012.  The rate to include cutting and welding or jointing with flanges as required and for coating and lining as per specifications.  Flanges according to Rand Water specification (DRG No. A11791)"]
[]
["14.2.2.1",null,"1832mm OD, straight pipe flanged on one end, 9520mm long, 16mm thick, with puddle flange placed at 1140mm from the flange (1)","No.",1]
[]
["14.2.2.2",null,"1832mm OD, straight pipe flanged on one end, 4580mm long, 16mm thick (4)","No.",1]
[]
["14.2.2.3",null,"1832 x 1424mm OD concentric reducer with 300mm extensions on either side, and flanged on the 1424mm OD side, 16mm thick (5)","No.",2]
[]
["14.2.2.4",null,"1832mm OD straight pipe, flanged on one end, 1780mm long, 16mm thick (7)","No.",1]
[]
["14.2.2.5",null,"1832mm OD straight pipe, flanged on one end, 2160mm long, 16mm thick with puddle flange placed at 1965mm from flange (9)","No.",1]
[]
["14.2.2.6",null,"1832mm OD straight pipe, 8190mm long, 16mm thick (10)","No.",1]
[]
[]
["Total brought forward "]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate","Amount"]
["Total Carried Forward  "]
["14.2.2.7",null,"1832mm OD, 16mm thick, 45 degree bend (11)","No.",1]
[]
["14.2.2.8",null,"1836mm OD straight pipe, 6000mm long with 718mm ID stub, 600mm long with flange and collar plate(see item 9.1.2.9) (12)","No.",1]
[]
["14.2.2.9",null,"6mm thick collar plate with 718mm ID & 1060mm OD (13)","No.",1]
[]
["14.2.2.10",null,"DN300 riser piece, flanged both ends. DN300 and DN800 Flanges (14)","No.",1]
[]
["14.2.2.11",null,"406.4mm OD straight pipe, 675mm long, 9.52mm thick (17)","No.",1]
[]
["14.2.2.12",null,"406.4mm OD, 9.52mm thick, 90 degree bend (18)","No.",3]
[]
["14.2.2.13",null,"406.4mm OD straight pipe, flanged on one end, 9.52mm thick, 500mm long (19)","No.",1]
[]
["14.2.2.14",null,"406.4mm OD straight pipe, flanged on one end, 9.52mm thick, 1600mm long (22)","No.",1]
[]
["14.2.2.15",null,"406.4mm OD straight pipe, 2995mm long, 9.52mm thick (23)","No.",1]
[]
["14.2.2.16",null,"406.4mm OD straight pipe, 1940mm long, 9.52mm thick (24)","No.",1]
[]
["14.2.2.17",null,"406.4mm OD, equal tee, 18mm thick (25)","No.",1]
[]
[]
[14.3,null,"PHASE 3: SHEET 1 OF 3 PIPE SPECIALS"]
[]
["14.3.1",null,"Manufacture and deliver the following pipe specials as per DRG No R0_9160/013.  The rate to include cutting and welding or jointing with flanges as required and for coating and lining as per specifications.  Flanges according to Rand Water specification (DRG No. A11791)"]
[]
["14.3.1.1",null,"1832mm OD, Straight pipe flanged on one end, 5830mm long, 16mm thick, with puddle flange placed at 1140mm from the flange (1)","No.",1]
[]
["14.3.1.2",null,"1832mm OD, Straight pipe flanged on one end, 1580mm long, 16mm thick, with puddle flange placed at 830mm from the flange (4)","No.",1]
[]
["14.3.1.3",null,"1832mm OD straight pipe, 9200mm long, 16mm thick (5)","No.",1]
[]
["14.3.1.4",null,"1832mm OD x 1424mm OD reducer with 300mm extensions on either sides, 16mm thick (6)","No.",1]
[]
["14.3.1.5",null,"1424mm OD, Straight pipe flanged on one end, 1700mm long, 12mm thick, with a puddle flange placed at 1000mm from the flange (7)","No.",1]
[]
[]
[]
["Total brought forward "]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate","Amount"]
["Total Carried Forward  "]
["14.3.1.6",null,"1832mm OD x 1424mm OD reducer with 300mm extensions on 1832mm OD side and 1440mm extension on the 1424mm OD side , 16mm thick, flanged on both ends (9)","No.",1]
[]
["14.3.1.7",null,"1832mm OD, Straight pipe flanged on one end, 5000mm long, 16mm thick, with a puddle flange placed at 2770mm from the flange (11)","No.",1]
[]
["14.3.1.8",null,"1832mm OD, 16mm thick, 45 degree bend (12)","No.",1]
[]
["14.3.1.9",null,"2032mm OD straight pipe, 3260mm long, 18mm thick (13)","No.",1]
[]
["14.3.1.10",null,"2032mm OD x 1832mm OD, un-equal tee, 18mm thick , with 2000 from 1832mm OD to center of 2024mm OD(14)","No.",1]
[]
["14.3.1.11",null,"2032mm OD straight pipe, 4900mm long, 18mm thick (15)","No.",1]
[]
["14.3.1.12",null,"2032mm OD x 1832mm OD, un-equal tee, 18mm thick , with 3560 from 1832mm OD to center of 2032mm OD(16)","No.",1]
[]
["14.3.1.13",null,"2036mm OD straight pipe, 18mm thick, 6800mm long with 816mm OD stub, placed 3800mm from the edge, 600mm long with flange and collar plate (17)","No.",1]
[]
["14.3.1.14",null,"DN300 riser piece, flanged both ends. DN300 and DN800 Flanges (18)","No.",1]
[]
["14.3.1.15",null,"406.4mm OD, 9.52mm thick,straight pipe, 675mm long  (21)","No.",1]
[]
["14.3.1.16",null,"406mm OD, 9.52mm thick, 90 degree bend (22)","No.",5]
[]
["14.3.1.17",null,"406mm OD, straight pipe, 9.52mm thick, flanged on one end, 500mm long. (23)","No.",1]
[]
["14.3.1.18",null,"406mm OD, straight pipe, 9.52mm thick, flanged on one end, 1500mm long. (26)","No.",1]
[]
["14.3.1.19",null,"406.4mm OD, 9.52mm thick, straight pipe, 2370mm long  (27)","No.",1]
[]
["14.3.1.20",null,"406.4mm OD, 9.52mm thick, straight pipe, 5700mm long  (28)","No.",1]
[]
["14.3.1.21",null,"406mm OD, 9.52mm thick, 45 degree bend (29)","No.",2]
[]
["14.3.1.22",null,"406.4mm OD, 9.52mm thick, straight pipe, 7150mm long  (30)","No.",1]
[]
["14.3.1.23",null,"406.4mm OD, 9.52mm thick, straight pipe, 6765mm long  (31)","No.",1]
[]
["14.3.1.24",null,"406.4mm OD, 9.52mm thick, straight pipe, 2630mm long  (32)","No.",1]
["Total brought forward "]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate","Amount"]
["Total Carried Forward  "]
["14.3.1.25",null,"406.4mm OD, 9.52mm thick, straight pipe, 2000mm long  (33)","No.",1]
[]
["14.3.1.26",null,"406.4mm OD, equal tee, 9.52mm thick (34)","No.",1]
[]
[]
["14.3.2",null,"Installation of Pipe specials"]
[null,null,"Collect and install the following pipe specials as per DRG No R0_9160/013.  The rate to include cutting and welding or jointing with flanges as required and for coating and lining as per specifications.  Flanges according to Rand Water specification (DRG No. A11791)"]
[null,null,"]"]
["14.3.2.1",null,"1832mm OD, Straight pipe flanged on one end, 5830mm long, 16mm thick, with puddle flange placed at 1140mm from the flange (1)","No.",1]
[]
["14.3.2.2",null,"1832mm OD, straight pipe flanged on one end, 1580mm long, 16mm thick, with puddle flange placed at 830mm from the flange (4)","No.",1]
[]
["14.3.2.3",null,"1832mm OD straight pipe, 9200mm long, 16mm thick (5)","No.",1]
[]
["14.3.2.4",null,"1832mm OD x 1424mm OD reducer with 300mm extensions on either sides, 16mm thick (6)","No.",1]
[]
["14.3.2.5",null,"1424mm OD, straight pipe flanged on one end, 1700mm long, 12mm thick, with a puddle flange placed at 1000mm from the flange (7)","No.",1]
[]
["14.3.2.6",null,"1832mm OD x 1424mm OD reducer with 300mm extensions on 1832mm OD side and 1440mm extension on the 1424mm OD side , 16mm thick, flanged on both ends (9)","No.",1]
[]
["14.3.2.7",null,"1832mm OD, straight pipe flanged on one end, 5000mm long, 16mm thick, with a puddle flange placed at 2770mm from the flange (11)","No.",1]
[]
["14.3.2.8",null,"1832mm OD, 16mm thick, 45 degree bend (12)","No.",1]
[]
["14.3.2.9",null,"2032mm OD straight pipe, 3260mm long, 18mm thick (13)","No.",1]
[]
["14.3.2.10",null,"2032mm OD x 1832mm OD, un-equal tee, 18mm thick , with 2000 from 1832mm OD to center of 2024mm OD(14)","No.",1]
[]
["14.3.2.11",null,"2032mm OD straight pipe, 4900mm long, 18mm thick (15)","No.",1]
[]
["14.3.2.12",null,"2032mm OD x 1832mm OD, un-equal tee, 18mm thick , with 3560 from 1832mm OD to center of 2032mm OD(16)","No.",1]
[]
["14.3.2.13",null,"2036mm OD straight pipe, 18mm thick, 6800mm long with 816mm OD stub, placed 3800mm from the edge, 600mm long with flange and collar plate (17)","No.",1]
[]
["Total brought forward "]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate"]
["Total Carried Forward  "]
["14.3.2.14",null,"DN300 riser piece, flanged both ends. DN300 and DN800 Flanges (18)","No.",1]
[]
["14.3.2.15",null,"406.4mm OD, 9.52mm thick,straight pipe, 675mm long  (21)","No.",1]
[]
["14.3.2.16",null,"406mm OD, 9.52mm thick, 90 degree bend (22)","No.",5]
[]
["14.3.2.17",null,"406mm OD, straight pipe, 9.52mm thick, flanged on one end, 500mm long. (23)","No.",1]
[]
["14.3.2.18",null,"406mm OD, straight pipe, 9.52mm thick, flanged on one end, 1500mm long. (26)","No.",1]
[]
["14.3.2.19",null,"406.4mm OD, 9.52mm thick, straight pipe, 2370mm long  (27)","No.",1]
[]
["14.3.2.20",null,"406.4mm OD, 9.52mm thick, straight pipe, 5700mm long  (28)","No.",1]
[]
["14.3.2.21",null,"406mm OD, 9.52mm thick, 45 degree bend (29)","No.",2]
[]
["14.3.2.22",null,"406.4mm OD, 9.52mm thick, straight pipe, 7150mm long  (30)","No.",1]
[]
["14.3.2.23",null,"406.4mm OD, 9.52mm thick, straight pipe, 6765mm long  (31)","No.",1]
[]
["14.3.2.24",null,"406.4mm OD, 9.52mm thick, straight pipe, 2630mm long  (32)","No.",1]
[]
["14.3.2.25",null,"406.4mm OD, 9.52mm thick, straight pipe, 2000mm long  (33)","No.",1]
[]
["14.3.2.26",null,"406.4mm OD, equal tee, 9.52mm thick (34)","No.",1]
[]
[]
[14.4,null,"PHASE 3: SHEET 2 OF 3 PIPE SPECIALS"]
[]
["14.4.1",null,"Manufacture and deliver the following pipe specials as per DRG No R0_9160/014.  The rate to include cutting and welding or jointing with flanges as required and for coating and lining as per specifications.  Flanges according to Rand Water specification (DRG No. A11791)"]
[]
["14.4.1.1",null,"2540mm OD x 2032mm OD reducer, 1400mm long with 300mm extension on either sides, 20mm thick (35)","No.",1]
[]
["14.4.1.2",null,"2032mm OD straight pipe, 18mm thick, flanged on one end , 2800mm long with a puddle flange placed 1900mm from the flange (36)","No.",2]
[]
["14.4.1.3",null,"219.1mm OD straight pipe, 1580mm long, flanged on one end, 7mm thick (38)","No.",1]
[]
["14.4.1.4",null,"219.1mm OD straight pipe, 7mm thick, flanged on one end , 2340mm long with a puddle flange placed 740mm from the flange (40)","No.",1]
[]
[]
["Total brought forward "]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate"]
["Total Carried Forward  "]
["14.4.1.5",null,"406mm OD x 219.1mm OD reducer, 9.52mm thick (41)","No.",1]
[]
["14.4.1.6",null,"406.4mm OD, 9.52mm Thick straight pipe, 3455mm long  (42)","No.",1]
[]
["14.4.1.7",null,"406mm OD, 9.52mm thick, 45 degree bend (43)","No.",1]
[]
["14.4.1.8",null,"406.4mm OD, 9.52mm Thick straight pipe, 1495mm long  (44)","No.",1]
[]
["14.4.1.9",null,"406.4mm OD, 9.52mm Thick straight pipe, 3100mm long  (45)","No.",4]
[]
["14.4.1.10",null,"406.4mm OD, 9.52mm Thick straight pipe, 24930mm long  (46)","No.",1]
[]
["14.4.1.11",null,"406.4mm OD, equal tee, 9.52mm thick (47)","No.",1]
[]
[]
["14.4.2",null,"Installation of Pipe specials"]
[null,null,"Collect and install the following pipe specials as per DRG No R0_9160/014.  The rate to include cutting and welding or jointing with flanges as required and for coating and lining as per specifications.  Flanges according to Rand Water specification (DRG No. A11791)"]
[]
["14.4.2.1",null,"2540mm OD x 2032mm OD reducer, 1400mm long with 300mm extension on either sides, 20mm thick (35)","No.",1]
[]
["14.4.2.2",null,"2032mm OD straight pipe, 18mm thick, flanged on one end , 2800mm long with a puddle flange placed 1900mm from the flange (36)","No.",2]
[]
["14.4.2.3",null,"219.1mm OD straight pipe, 1580mm long, flanged on one end, 7mm thick (38)","No.",1]
[]
["14.4.2.4",null,"219.1mm OD straight pipe, 7mm thick, flanged on one end , 2340mm long with a puddle flange placed 740mm from the flange (40)","No.",1]
[]
[]
[14.5,null,"PHASE 4: SHEET 3 OF 3 PIPE SPECIALS"]
[]
["14.5.1",null,"Manufacture and deliver the following pipe specials as per DRG No R0_9160/015.  The rate to include cutting and welding or jointing with flanges as required and for coating and lining as per specifications.  Flanges according to Rand Water specification (DRG No. A11791)"]
[]
["14.5.1.1",null,"1832mm OD, 16mm Thick straight pipe, 16000mm long  (48)","No.",1]
[]
["14.5.1.2",null,"1832mm OD, straight pipe, 16mm thick, flanged on one end, 2850mm long, with a puddle placed 1125mm from the flange (49)","No.",1]
["Total brought forward "]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate"]
["Total Carried Forward  "]
["14.5.1.3",null,"∅1832 mm OD. x ∅1832 mm OD x 5015 mm long tee with one flange and 2070 with plain end, 3115mm from the flange to the center of the tee, 16mm thick. with a puddle flange placed 1015mm from the flange (52) \n","No.",1]
[]
["14.5.1.4",null,"1832mm OD, 16mm Thick straight pipe, 7000mm long  (53)","No.",1]
[]
["14.5.1.5",null,"1832mm OD x 1424mm OD concentric reducer, with 300mm extensions on either side, 16mm thick (54)","No.",1]
[]
["14.5.1.6",null,"1832mm OD, straight pipe, 16mm thick, flanged on one end, 2100mm long, with a puddle placed 1405mm from the flange (55)","No.",1]
[]
["14.5.1.7",null,"1832mm OD x 1424mm OD reducer with 300mm and 1530mm extensions on eithe sides, flanged on both ends, 16mm thick. (57)","No.",1]
[]
["14.5.1.8",null,"1832mm OD, straight pipe, 16mm thick, flanged on one end, 4700mm long, with a puddle placed 1125mm from the flange (59)","No.",1]
[]
["14.5.1.9",null,"1832mm OD 45 degree bend, 16mm thick. (60)","No.",1]
[]
["14.5.1.10",null,"2036mm OD x 1832mm OD unequal tee, plain ends, 18mm thick. (61)","No.",1]
[]
["14.5.1.11",null,"406.3mm OD, straight pipe, plain ends and 880mm long. (62)","No.",1]
[]
["14.5.1.12",null,"406.3mm OD 90 degree bend, 9.52mm thick. (63)","No.",1]
[]
["14.5.1.13",null,"406.3mm OD, straight pipe, flanged on one end and 480mm long. (64)","No.",1]
[]
["14.5.1.14",null,"406.3mm OD, straight pipe, flanged on one end and 3920mm long. (67)","No.",1]
[]
["14.5.1.15",null,"406.3mm OD, straight pipe, plain ends and 2085mm long. (68)","No.",1]
[]
["14.5.1.16",null,"406.3mm OD 20 degree bend, 9.52mm thick. (69)","No.",2]
[]
["14.5.1.17",null,"406.3mm OD, straight pipe, flanged on one end and 1650mm long. (70)","No.",1]
[]
["14.5.1.18",null,"406.3mm OD, straight pipe, flanged on one end and 2820mm long. (71)","No.",1]
[]
["14.5.1.19",null,"406.3mm OD equal tee piece, 9.52mm thick, plain ends. (72)","No.",1]
[]
[]
[]
[]
[]
["Total brought forward "]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate"]
["Total Carried Forward  "]
["14.5.2",null,"Installation of Pipe specials"]
[null,null,"Collect and install the following pipe specials as per DRG No R0_9160/015.  The rate to include cutting and welding or jointing with flanges as required and for coating and lining as per specifications.  Flanges according to Rand Water specification (DRG No. A11791)"]
[]
["14.5.2.1",null,"1832mm OD, 16mm Thick straight pipe, 16000mm long  (48)","No.",1]
[]
["14.5.2.2",null,"1832mm OD, straight pipe, 16mm thick, flanged on one end, 2850mm long, with a puddle placed 1125mm from the flange (49)","No.",1]
[]
["14.5.2.3",null,"∅1832 mm OD. x ∅1832 mm OD x 5015 mm long tee with one flange and 2070 with plain end, 3115mm from the flange to the center of the tee, 16mm thick. with a puddle flange placed 1015mm from the flange (52) \n","No.",1]
[]
["14.5.2.4",null,"1832mm OD, 16mm Thick straight pipe, 7000mm long  (53)","No.",1]
[]
["14.5.2.5",null,"1832mm OD x 1424mm OD concentric reducer, with 300mm extensions on either side, 16mm thick (54)","No.",1]
[]
["14.5.2.6",null,"1832mm OD, straight pipe, 16mm thick, flanged on one end, 2100mm long, with a puddle placed 1405mm from the flange (55)","No.",1]
[]
["14.5.2.7",null,"1832mm OD x 1424mm OD reducer with 300mm and 1530mm extensions on eithe sides, flanged on both ends, 16mm thick. (57)","No.",1]
[]
["14.5.2.8",null,"1832mm OD, straight pipe, 16mm thick, flanged on one end, 4700mm long, with a puddle placed 1125mm from the flange (59)","No.",1]
[]
["14.5.2.9",null,"1832mm OD 45 degree bend, 16mm thick. (60)","No.",1]
[]
["14.5.2.10",null,"2036mm OD x 1832mm OD unequal tee, plain ends, 18mm thick. (61)","No.",1]
[]
["14.5.2.11",null,"406.3mm OD, straight pipe, plain ends and 880mm long. (62)","No.",1]
[]
["14.5.2.12",null,"406.3mm OD 90 degree bend, 9.52mm thick. (63)","No.",1]
[]
["14.5.2.13",null,"406.3mm OD, straight pipe, flanged on one end and 480mm long. (64)","No.",1]
[]
["14.5.2.14",null,"406.3mm OD, straight pipe, flanged on one end and 3920mm long. (67)","No.",1]
[]
["14.5.2.15",null,"406.3mm OD, straight pipe, plain ends and 2085mm long. (68)","No.",1]
[]
["14.5.2.16",null,"406.3mm OD 20 degree bend, 9.52mm thick. (69)","No.",2]
[]
["Total brought forward "]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate"]
["Total Carried Forward  "]
["14.5.2.17",null,"406.3mm OD, straight pipe, flanged on one end and 1650mm long. (70)","No.",1]
[]
["14.5.2.18",null,"406.3mm OD, straight pipe, flanged on one end and 2820mm long. (71)","No.",1]
[]
["14.5.2.19",null,"406.3mm OD equal tee piece, 9.52mm thick, plain ends. (72)","No.",1]
[]
[]
[14.6,null,"PHASE 1B: PIPE SPECIALS"]
[]
["14.6.1",null,"Manufacture and deliver the following pipe specials as per DRG No R0_9160/016.  The rate to include cutting and welding or jointing with flanges as required and for coating and lining as per specifications.  Flanges according to Rand Water specification (DRG No. A11791)"]
[]
["14.6.1.1",null,"1832mm OD x 609.1mm OD concentric reducer with 300mm long extensions on either sides, 18mm thick (73)","No.",1]
[]
["14.6.1.2",null,"609.6mm OD, dome, 425mm long. (74)","No.",1]
[]
["14.6.1.3",null,"1832mm OD, straight pipe, 8000mm long, 16mm thick. (76)","No.",1]
[]
["14.6.1.4",null,"1832mm OD, 22 degree bend with 800mm extension straight pipe on one end, 16mm thick. (77)","No.",1]
[]
["14.6.1.5",null,"1832mm OD x 1424mm OD concetric reducer, 16mm thick with 300mm long extensions on eighter sides. (78)","No.",1]
[]
["14.6.1.6",null,"1424mm OD straight pipe, 2100mm long, flanged on one end with a puddle flange placed 1400mm away from the flange, 12mm thick. (79) ","No.",1]
[]
["149.6.1.7",null,"1832mm OD x 1424mm OD concetric reducer, 16mm thick with 300mm long extension on the 1832mm OD side and 1530mm long extension on the 1424mm OD sides, flanged on both ends. (81)","No.",1]
[]
["14.6.1.8",null,"1832mm OD straight pipe, 5000mm long, flanged on one end with a puddle flange placed 3480mm away from the flange, 16mm thick. (84) ","No.",1]
[]
["14.6.1.9",null,"1832mm OD straight pipe with plain ends, 3780mm long, 16mm thick. (85)","No.",1]
[]
["14.6.1.10",null,"324mm OD riser piece flanged with DN300 flange on one end and DN700 on the other end, 7mm thick. (87)","No.",1]
[]
["14.6.1.11",null,"1832mm OD straight pipe, 3780mm long with 714mm OD, 600mm long stub with a flange at the end, 16mm thick. (90)","No.",1]
[]
[]
[]
["Total brought forward "]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate"]
["Total Carried Forward  "]
["14.6.1.12",null,"1832mm OD straight pipe, 20920mm long, 16mm thick. (91)","No.",1]
[]
["14.6.1.13",null,"406.3mm OD straight pipe, 900mm long, 9.52mm thick. (92)","No.",1]
[]
["14.6.1.14",null,"406.3mm OD 90 degree bend, 9.52mm thick. (93)","No.",2]
[]
["14.6.1.15",null,"406.3mm OD straight pipe, 480mm long, 9.52mm thick, flanged on one end (94)","No.",1]
[]
["14.6.1.16",null,"406.3mm OD straight pipe, 4100mm long, flanged on one end. (97)","No.",1]
[]
["14.6.1.17",null,"406.3mm OD straight pipe, 10000mm long. 9.52mm thick(98)","No.",1]
[]
["14.6.1.18",null,"1832mm OD, 16mm thick, 20 degree bend. (99)","No.",1]
[]
["14.6.1.19",null,"1832mm OD straight pipe, 32870mm long. 16mm thick(100)","No.",1]
[]
["14.6.1.20",null,"1832mm OD, 16mm thick, 90 degree bend. (101)","No.",1]
[]
["14.6.1.21",null,"1832mm OD straight pipe, 14970mm long. 16mm thick(102)","No.",1]
[]
["14.6.1.22",null,"2524mm OD x 1832mm OD, un-equal tee piece, 16mm thick. (103)","No.",1]
[]
["14.6.1.23",null,"2524mm OD straight pipe, 16mm thick and 1900mm long, with a puddle flange placed 1190mm away from the flange. (104)","No.",2]
[]
[]
["14.6.2",null,"Installation of Pipe specials"]
[null,null,"Collect and install the following pipe specials as per DRG No R0_9160/016.  The rate to include cutting and welding or jointing with flanges as required and for coating and lining as per specifications.  Flanges according to Rand Water specification (DRG No. A11791)"]
[]
["14.6.2.1",null,"1832mm OD x 609.1mm OD concentric reducer with 300mm long extensions on either sides, 18mm thick (73)","No.",1]
[]
["14.6.2.2",null,"609.6mm OD, dome, 425mm long. (74)","No.",1]
[]
["14.6.2.3",null,"1832mm OD, straight pipe, 8000mm long, 16mm thick. (76)","No.",1]
[]
["14.6.2.4",null,"1832mm OD, 22 degree bend with 800mm extension straight pipe on one end, 16mm thick. (77)","No.",1]
[]
["14.6.2.5",null,"1832mm OD x 1424mm OD concetric reducer, 16mm thick with 300mm long extensions on eighter sides. (78)","No.",1]
["Total brought forward "]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate"]
["Total Carried Forward  "]
["14.6.2.6",null,"1424mm OD straight pipe, 2100mm long, flanged on one end with a puddle flange placed 1400mm away from the flange, 12mm thick. (79) ","No.",1]
[]
["14.6.2.7",null,"1832mm OD x 1424mm OD concetric reducer, 16mm thick with 300mm long extension on the 1832mm OD side and 1530mm long extension on the 1424mm OD sides, flanged on both ends. (81)","No.",1]
[]
["14.6.2.8",null,"1832mm OD straight pipe, 5000mm long, flanged on one end with a puddle flange placed 3480mm away from the flange, 16mm thick. (84) ","No.",1]
[]
["14.6.2.9",null,"1832mm OD straight pipe with plain ends, 3780mm long, 16mm thick. (85)","No.",1]
[]
["14.6.2.10",null,"324mm OD riser piece flanged with DN300 flange on one end and DN700 on the other end, 7mm thick. (87)","No.",1]
[]
["14.6.2.11",null,"1832mm OD straight pipe, 3780mm long with 714mm OD, 600mm long stub with a flange at the end, 16mm thick. (90)","No.",1]
[]
["14.6.2.12",null,"1832mm OD straight pipe, 20920mm long, 16mm thick. (91)","No.",1]
[]
["14.6.2.13",null,"406.3mm OD straight pipe, 900mm long, 9.52mm thick. (92)","No.",1]
[]
["14.6.2.14",null,"406.3mm OD 90 degree bend, 9.52mm thick. (93)","No.",2]
[]
["14.6.2.15",null,"406.3mm OD straight pipe, 480mm long, 9.52mm thick, flanged on one end (94)","No.",1]
[]
["14.6.2.16",null,"406.3mm OD straight pipe, 4100mm long, flanged on one end. (97)","No.",1]
[]
["14.6.2.17",null,"406.3mm OD straight pipe, 10000mm long. 9.52mm thick(98)","No.",1]
[]
["14.6.2.18",null,"1832mm OD, 16mm thick, 20 degree bend. (99)","No.",1]
[]
["14.6.2.19",null,"1832mm OD straight pipe, 32870mm long. 16mm thick(100)","No.",1]
[]
["14.6.2.20",null,"1832mm OD, 16mm thick, 90 degree bend. (101)","No.",1]
[]
["14.6.2.21",null,"1832mm OD straight pipe, 14970mm long. 16mm thick(102)","No.",1]
[]
["14.6.2.22",null,"2524mm OD x 1832mm OD, un-equal tee piece, 16mm thick. (103)","No.",1]
[]
["14.6.2.23",null,"2524mm OD straight pipe, 16mm thick and 1900mm long, with a puddle flange placed 1190mm away from the flange. (104)","No.",2]
[]
[]
["Total brought forward "]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate"]
["Total Carried Forward  "]
[]
[14.7,null,"PIPE SPECIALS FOR PUMPSETS START"]
["14.7.1",null,"Manufacture and deliver the following pipe specials as per DRG No R0_9160/010.  The rate to include cutting and welding or jointing with flanges as required and for coating and lining as per specifications.  Flanges according to Rand Water specification (DRG No. A11791)"]
[]
["14.7.1.1",null,"1424mm OD, 16mm thick, 3575mm long with a pressure ring placed 2367mm away from flange. (1)","No.",4]
[]
["14.7.1.2",null,"1424mm OD x 1224mm OD reducer, 14mm thick. (2)","No.",8]
[]
["14.7.1.3",null,"1220mm OD 45 degree bend, 10mm thick. (3)","No.",4]
[]
["14.7.1.4",null,"1220 mm OD straight pipe, 3540mm long, 10mm thick. (4)","No.",4]
[]
["14.7.1.5",null,"1424 mm OD straight pipe, 3010mm long, 14mm thick. (5)","No.",4]
[]
["14.7.1.6",null,"1424mm OD 45 degree bend, 14mm thick. (6)","No.",4]
[]
["14.7.1.7",null,"1832mm OD x 1424mm OD reducer, 18mm thick (7)","No.",4]
[]
[]
["14.7.2",null,"Installation of Pipe specials"]
[null,null,"Collect and install the following pipe specials as per DRG No R0_9160/010.  The rate to include cutting and welding or jointing with flanges as required and for coating and lining as per specifications.  Flanges according to Rand Water specification (DRG No. A11791)"]
[]
["14.7.2.1",null,"1424mm OD, 16mm thick, 3575mm long with a pressure ring placed 2367mm away from flange. (1)","No.",4]
[]
["14.7.2.2",null,"1424mm OD x 1224mm OD reducer, 14mm thick. (2)","No.",8]
[]
["14.7.2.3",null,"1220mm OD 45 degree bend, 10mm thick. (3)","No.",4]
[]
["14.7.2.4",null,"1220 mm OD straight pipe, 3540mm long, 10mm thick. (4)","No.",4]
[]
["14.7.2.5",null,"1424 mm OD straight pipe, 3010mm long, 14mm thick. (5)","No.",4]
[]
["14.7.2.6",null,"1424mm OD 45 degree bend, 14mm thick. (6)","No.",4]
[]
["14.7.2.7",null,"1832mm OD x 1424mm OD reducer, 18mm thick (7)","No.",4]
[]
["Total brought forward "]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate"]
["Total Carried Forward  "]
[14.8,null,"Valves"]
["14.8.1",null,"Phase 1: VALVES"]
[null,null,"Manufacture and deliver the following pipe specials as per DRG No R0_9160/011.  The rate to include cutting and welding or jointing with flanges as required and for coating and lining as per specifications.  Flanges according to Rand Water specification (DRG No. A11791)"]
[]
["14.8.1.1",null,"DN 1400 Non return valve, electrically actuated (5000KPa)(6)","N0",1]
[]
["14.8.1.2",null,"DN 1800 Butterfly valve, electrically actuated (3500KPa)(8)","No ",1]
[]
["14.8.1.3",null,"DN 300mm gate valve for air valve (3500KPa)(14)","No",2]
[]
["14.8.1.4",null,"DN 2000 Butterfly valve, electrically actuated(3500KPa)(24)","No ",2]
[]
["14.8.1.5",null,"DN 400 sluice gate valve (3500KPa)(88)","No ",1]
[]
["14.8.1.6",null,"DN 400 Surge anticipation valve (3500KPa)(89)","No ",1]
[]
[]
["14.8.2",null,"Installation of phase 1 Valves"]
[null,null,"Collect and install the following valves as per DRG No R0_9160/011.  The rate to include cutting and welding or jointing with flanges as required and for coating and lining as per specifications.  Flanges according to Rand Water specification (DRG No. A11791)"]
[]
["14.8.2.1",null,"DN 1400 Non return valve, electrically actuated (5000KPa)(6)","N0",1]
[]
["14.8.2.2",null,"DN 1800 Butterfly valve, electrically actuated (3500KPa)(8)","No ",1]
[]
["14.8.2.3",null,"DN 300mm gate valve for air valve (3500KPa)(14)","No",2]
[]
["14.8.2.4",null,"DN 2000 Butterfly valve, electrically actuated(3500KPa)(24)","No ",2]
[]
["14.8.2.5",null,"DN 400 sluice gate valve (3500KPa)(88)","No ",1]
[]
["14.8.2.6",null,"DN 400 Surge anticipation valve (3500KPa)(89)","No ",1]
{"$rows_empty":10}
["Total brought forward "]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate"]
["Total Carried Forward  "]
["14.8.3",null,"Phase 2: VALVES"]
[null,null,"Manufacture and deliver the following pipe specials as per DRG No R0_9160/012.  The rate to include cutting and welding or jointing with flanges as required and for coating and lining as per specifications.  Flanges according to Rand Water specification (DRG No. A11791)"]
[]
["14.8.3.1",null,"DN 1400 Non return valve, electrically actuated (5000KPa)(6)","No.",1]
[]
["14.8.3.2",null,"DN 1800 Butterfly valve, electrically actuated (3500KPa)(8)","No.",1]
[]
["14.8.3.3",null,"DN 300mm gate valve for air valve (3500KPa)(15)","No.",1]
[]
["14.8.3.4",null,"DN 400 sluice gate valve (3500KPa)(20)","No.",1]
[]
["14.8.3.5",null,"DN 400 Surge anticipation valve (3500KPa)(21)","No ",1]
[]
[]
["14.8.4",null,"Installation of phase 2 Valves"]
[null,null,"Collect and install the following valves as per DRG No R0_9160/012.  The rate to include cutting and welding or jointing with flanges as required and for coating and lining as per specifications.  Flanges according to Rand Water specification (DRG No. A11791)"]
[]
["14.8.4.1",null,"DN 1400 Non return valve, electrically actuated (5000KPa)(6)","No.",1]
[]
["14.8.4.2",null,"DN 1800 Butterfly valve, electrically actuated (3500KPa)(8)","No.",1]
[]
["14.8.4.3",null,"DN 300mm gate valve for air valve (3500KPa)(15)","No.",1]
[]
["14.8.4.4",null,"DN 400 sluice gate valve (3500KPa)(20)","No.",1]
[]
["14.8.4.5",null,"DN 400 Surge anticipation valve (3500KPa)(21)","No ",1]
[]
[]
["14.8.5",null,"Phase 3: SHEET 1 OF 3 VALVES"]
[null,null,"Manufacture and deliver the following pipe specials as per DRG No R0_9160/013.  The rate to include cutting and welding or jointing with flanges as required and for coating and lining as per specifications.  Flanges according to Rand Water specification (DRG No. A11791)"]
[]
["14.8.5.1",null,"DN 1400 Non return valve, electrically actuated (5000KPa)(8)","No ",1]
[]
["14.8.5.2",null,"DN 1800 Butterfly valve, electrically actuated (3500KPa)(10)","No ",1]
[]
["14.8.5.3",null,"DN 300mm gate valve for air valve (3500KPa)(19)","No ",1]
[]
["Total brought forward "]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate"]
["Total Carried Forward  "]
["14.8.5.4",null,"DN 400 sluice gate valve (3500KPa)(24)","No ",1]
[]
["14.8.5.5",null,"DN 400 Surge anticipation valve (3500KPa)(25)","No ",1]
[]
[]
["14.8.6",null,"Installation of phase 3 SHEET 1 OF 3 Valves"]
[null,null,"Collect and install the following valves as per DRG No R0_9160/013.  The rate to include cutting and welding or jointing with flanges as required and for coating and lining as per specifications.  Flanges according to Rand Water specification (DRG No. A11791)"]
[]
["14.8.6.1",null,"DN 1400 Non return valve, electrically actuated (5000KPa)(8)","No ",1]
[]
["14.8.6.2",null,"DN 1800 Butterfly valve, electrically actuated (3500KPa)(10)","No ",1]
[]
["14.8.6.3",null,"DN 300mm gate valve for air valve (3500KPa)(19)","No ",1]
[]
["14.8.6.4",null,"DN 400 sluice gate valve (3500KPa)(24)","No ",1]
[]
["14.8.6.5",null,"DN 400 Surge anticipation valve (3500KPa)(25)","No ",1]
[]
[]
["14.8.7",null,"Phase 3: SHEET 2 OF 3 VALVES"]
[null,null,"Manufacture and deliver the following pipe specials as per DRG No R0_9160/014.  The rate to include cutting and welding or jointing with flanges as required and for coating and lining as per specifications.  Flanges according to Rand Water specification (DRG No. A11791)"]
[]
["14.8.7.1",null,"DN 1800 Butterfly valve, electrically actuated (3500KPa)(37)","No ",1]
[]
["14.8.7.2",null,"DN 200mm gate scour valve (3500KPa)(39)","No ",1]
[]
[]
["14.8.8",null,"Installation of phase 3 SHEET 2 OF 3 Valves"]
[null,null,"Collect and install the following valves as per DRG No R0_9160/014.  The rate to include cutting and welding or jointing with flanges as required and for coating and lining as per specifications.  Flanges according to Rand Water specification (DRG No. A11791)"]
[]
["14.8.8.1",null,"DN 1800 Butterfly valve, electrically actuated (3500KPa)(37)","No ",1]
[]
["14.8.8.2",null,"DN 200mm gate scour valve (3500KPa)(39)","No ",1]
[]
[]
[]
[]
[]
["Total brought forward "]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate"]
["Total Carried Forward  "]
["14.8.9",null,"Phase 4: SHEET 3 OF 3 VALVES"]
[null,null,"Manufacture and deliver the following pipe specials as per DRG No R0_9160/015.  The rate to include cutting and welding or jointing with flanges as required and for coating and lining as per specifications.  Flanges according to Rand Water specification (DRG No. A11791)"]
[]
["14.8.9.1",null,"DN 1400 Non return valve, electrically actuated (5000KPa)(56)","No ",1]
[]
["14.8.9.2",null,"DN 1800 Butterfly valve, electrically actuated (3500KPa)(58)","No ",1]
[]
["14.8.9.3",null,"DN 400 sluice gate valve (3500KPa)(65)","No ",1]
[]
["14.8.9.4",null,"DN 400 Surge anticipation valve (3500KPa)(66)","No ",1]
[]
["14.8.10",null,"Installation of phase 4 SHEET 3 OF 3 Valves"]
[null,null,"Collect and install the following valves as per DRG No R0_9160/015.  The rate to include cutting and welding or jointing with flanges as required and for coating and lining as per specifications.  Flanges according to Rand Water specification (DRG No. A11791)"]
[]
["14.8.10.1",null,"DN 1400 Non return valve, electrically actuated (5000KPa)(56)","No ",1]
[]
["14.8.10.2",null,"DN 1800 Butterfly valve, electrically actuated (3500KPa)(58)","No ",1]
[]
["14.8.10.3",null,"DN 400 sluice gate valve (3500KPa)(65)","No ",1]
[]
["14.8.10.4",null,"DN 400 Surge anticipation valve (3500KPa)(66)","No ",1]
[]
["14.8.11",null,"Phase 1B: VALVES"]
[null,null,"Manufacture and deliver the following pipe specials as per DRG No R0_9160/016.  The rate to include cutting and welding or jointing with flanges as required and for coating and lining as per specifications.  Flanges according to Rand Water specification (DRG No. A11791)"]
[]
["14.8.11.1",null,"DN 1400 Non return valve, electrically actuated (5000KPa)(80)","No ",1]
[]
["14.8.11.2",null,"DN 1800 Butterfly valve, electrically actuated (3500KPa)(83)","No ",1]
[]
["14.8.11.3",null,"DN 300mm gate valve for air valve (3500KPa)(88)","No ",1]
[]
["14.8.11.4",null,"DN 400 sluice gate valve (3500KPa)(95)","No ",1]
["14.8.11.5",null,"DN 400 Surge anticipation valve (3500KPa)(96)","No ",1]
[]
["Total brought forward "]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate"]
["Total Carried Forward  "]
["14.8.12",null,"Installation of phase 1B Valves"]
[null,null,"Collect and install the following valves as per DRG No R0_9160/016.  The rate to include cutting and welding or jointing with flanges as required and for coating and lining as per specifications.  Flanges according to Rand Water specification (DRG No. A11791)"]
[]
["14.8.12.1",null,"DN 1400 Non return valve, electrically actuated (5000KPa)(80)","No ",1]
[]
["14.8.12.2",null,"DN 1800 Butterfly valve, electrically actuated (3500KPa)(83)","No ",1]
[]
["14.8.12.3",null,"DN 300mm gate valve for air valve (3500KPa)(88)","No ",1]
[]
["14.8.12.4",null,"DN 400 sluice gate valve (3500KPa)(95)","No ",1]
[]
["14.8.12.5",null,"DN 400 Surge anticipation valve (3500KPa)(96)","No ",1]
[]
[]
[14.9,null,"ELECTROMAGNETIC FLOWMETERS"]
[null,null,"Collect magnetic flowmeters from Rand Water Central Depot and as per the following diameters and pressure ratings to Rand Water Specifications (Refer to Dwg A11791), including installation, fitting, tightening and setting of gasket rings, flange bolts, nuts and washers:"]
[]
[]
["14.9.1",null,"PHASE 1 ELECTROMAGNETIC FLOWMETERS, REFER to drg no.RO_9160/011"]
[]
["14.9.1.1",null,"DN 1800 Electromagnetic flow meter 3500(Kpa)(2)","No ",1]
[]
["14.9.1.2",null,"DN 1800 Dismantling Joint (3500KPa)(3)","No ",2]
[]
[]
["14.9.2",null,"PHASE 2 ELECTROMAGNETIC FLOWMETERS, REFER to drg no.RO_9160/012"]
[]
["14.9.2.1",null,"DN 1800 Electromagnetic flow meter 3500(Kpa)(2)","No ",1]
[]
["14.9.2.2",null,"DN 1800 Dismantling Joint (3500KPa)(3)","No ",2]
[]
[]
["14.9.3",null,"PHASE 3 sheet 1 of 3 ELECTROMAGNETIC FLOWMETERS, REFER to drg no.RO_9160/013"]
[]
["14.9.3.1",null,"DN 1800 Electromagnetic flow meter 3500(Kpa)(2)","No ",1]
[]
["14.9.3.2",null,"DN 1800 Dismantling Joint (3500KPa)(3)","No ",2]
{"$rows_empty":7}
["Total brought forward "]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate"]
["Total Carried Forward  "]
["14.9.4",null,"PHASE 4 sheet 3 of 3 ELECTROMAGNETIC FLOWMETERS, REFER to drg no.RO_9160/015"]
[]
["14.9.4.1",null,"DN 1800 Electromagnetic flow meter 3500(Kpa)(50)","No ",1]
[]
["14.9.4.2",null,"DN 1800 Dismantling Joint (3500KPa)(51)","No ",2]
[]
[]
["14.9.5",null,"PHASE 1B ELECTROMAGNETIC FLOWMETERS, REFER to drg no.RO_9160/016"]
[]
["14.9.5.1",null,"DN 1800 Dismantling Joint (3500KPa)(82)","No ",1]
[]
["14.9.5.2",null,"DN 2500 Dismantling Joint (3500KPa)(106)","No ",1]
[]
["14.9.5.3",null,"DN 2500 Electromagnetic flow meter 3500(Kpa)(105)","No ",1]
[]
[]
["14.10.",null,"AIR VALVES"]
[null,null,"Collect Air valves from Rand Water Central Depot and as per the following diameters and pressure ratings to Rand Water Specifications (Refer to Dwg A11791), including installation, fitting, tightening and setting of gasket rings, flange bolts, nuts and washers:"]
[]
["14.10.1",null,"DN 300mm air valve (3500KPa), REFER to drg no. RO_9160/011 (15)","No ",2]
[]
["14.10.2",null,"DN 300mm air valve (3500KPa), REFER to drg no. RO_9160/012 (16)","No ",1]
[]
["14.10.3",null,"DN 300mm air valve (3500KPa), REFER to drg no. RO_9160/013 (20)","No ",1]
[]
["14.10.8",null,"DN 300mm air valve (3500KPa), REFER to drg no. RO_9160/016 (89)","No ",1]
[]
[]
["14.11.",null,"New additional air valves specials for B5 , B11 & B19 REFER to drg. No. RO_9160/019"]
["14.11.1",null,"Manufacture and deliver the following pipe specials as per DRG No R0_9160/019.  The rate to include cutting and welding or jointing with flanges as required and for coating and lining as per specifications.  Flanges according to Rand Water specification (DRG No. A11791)"]
[]
[null,null,"REFER TO TABLE 1"]
[]
["14.11.1.1",null,"1200mm OD compensation plate, 10mm thick (1)","No.",17]
[]
["14.11.1.2",null,"816mm OD straight pipe, 8mm thick, flanged on one ends (2)","No.",17]
[]
["14.11.1.3",null,"323.8mm OD straight riser pipe, 9.52mm thick, flanged on both ends (3)","No.",17]
[]
[]
["Total brought forward "]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate"]
["Total Carried Forward  "]
["14.11.1.4",null,"DN300 gate valve flanged on both ends (4)","No.",17]
[]
["14.11.1.5",null,"DN300 Air valve (5)","No.",17]
[]
[null,null,"REFER TO TABLE 2"]
[]
["14.11.1.6",null,"1480mm OD compensation plate, 25mm thick (1)","No.",2]
[]
["14.11.1.7",null,"1020mm OD straight pipe, 9.52mm thick, flanged on one ends (2)","No.",2]
[]
["14.11.1.8",null,"323.8mm OD straight riser pipe, 9.52mm thick, flanged on both ends (3)","No.",2]
[]
["14.11.1.9",null,"DN300 gate valve flanged on both ends (4)","No.",2]
[]
["14.11.1.10",null,"DN300 Air valve (5)","No.",2]
[]
["14.11.1.11",null,"8mm wrapper plate on B11 stiffened pipeline (6)","No.",2]
[]
[]
["14.11.2",null,"Installation of Pipe specials"]
[null,null,"Collect and install the following pipe specials as per DRG No R0_9160/019.  The rate to include cutting and welding or jointing with flanges as required and for coating and lining as per specifications.  Flanges according to Rand Water specification (DRG No. A11791)"]
[]
[null,null,"REFER TO TABLE 1"]
[]
["14.11.2.1",null,"1200mm OD compensation plate, 10mm thick (1)","No.",17]
[]
["14.11.2.2",null,"816mm OD straight pipe, 8mm thick, flanged on one ends (2)","No.",17]
[]
["14.11.2.3",null,"323.8mm OD straight riser pipe, 9.52mm thick, flanged on both ends (3)","No.",17]
[]
["14.11.2.4",null,"DN300 gate valve flanged on both ends (4)","No.",17]
[]
["14.11.2.5",null,"DN300 Air valve (5)","No.",17]
[]
[null,null,"REFER TO TABLE 2"]
[]
["14.11.2.6",null,"1480mm OD compensation plate, 25mm thick (1)","No.",2]
[]
["14.11.2.7",null,"1020mm OD straight pipe, 9.52mm thick, flanged on one ends (2)","No.",2]
[]
["14.11.2.8",null,"323.8mm OD straight riser pipe, 9.52mm thick, flanged on both ends (3)","No.",2]
["Total brought forward "]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate"]
["Total Carried Forward  "]
[]
["14.11.2.9",null,"DN300 gate valve flanged on both ends (4)","No.",2]
[]
["14.11.2.10",null,"DN300 Air valve (5)","No.",2]
[]
["14.11.2.11",null,"8mm wrapper plate on B11 stiffened pipeline (6)","No.",2]
[14.12,null,"New air valves replacing the existing for B5 & B11, REFER to drg no. RO_9160/018"]
["14.12.1",null,"Manufacture and deliver the following pipe specials as per DRG No R0_9160/018.  The rate to include cutting and welding or jointing with flanges as required and for coating and lining as per specifications.  Flanges according to Rand Water specification (DRG No. A11791)"]
[]
[]
[null,null,"REFER TO TABLE 1"]
[]
["14.12.1.1",null,"1450mm OD compensation plate, 16mm thick (1)","No.",6]
[]
["14.12.1.2",null,"610mm OD straight pipe, 9.5mm thick, flanged on one ends (2)","No.",6]
[]
["14.12.1.3",null,"323.8mm OD straight riser pipe, 9.52mm thick, flanged on both ends (3)","No.",6]
[]
["14.12.1.4",null,"DN300 gate valve flanged on both ends (4)","No.",6]
[]
["14.12.1.5",null,"DN300 Air valve (5)","No.",6]
[]
[null,null,"REFER TO TABLE 2"]
[]
["14.12.1.6",null,"1200mm OD compensation plate, 10mm thick (1)","No.",18]
[]
["14.12.1.7",null,"816mm OD straight pipe, 8mm thick, flanged on one ends (2)","No.",18]
[]
["14.12.1.8",null,"323.8mm OD straight riser pipe, 9.52mm thick, flanged on both ends (3)","No.",18]
[]
["14.12.1.9",null,"DN300 gate valve flanged on both ends (4)","No.",18]
[]
["9.12.1.10",null,"DN300 Air valve (5)","No.",18]
[]
[null,null,"REFER TO TABLE 3"]
[]
["14.12.1.11",null,"1480mm OD compensation plate, 25mm thick (1)","No.",13]
[]
["14.12.1.12",null,"1020mm OD straight pipe, 9.52mm thick, flanged on one ends (2)","No.",13]
[]
["9.12.1.13",null,"323.8mm OD straight riser pipe, 9.52mm thick, flanged on both ends (3)","No.",13]
[]
["14.12.1.14",null,"DN300 gate valve flanged on both ends (4)","No.",13]
[]
["Total brought forward "]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate"]
["Total Carried Forward  "]
["14.12.1.15",null,"DN300 Air valve (5)","No.",13]
[]
["14.12.1.16",null,"8mm wrapper plate on B11 stiffened pipeline","No.",13]
[]
["14.12.2",null,"Installation of Pipe specials"]
[null,null,"Collect and install the following pipe specials as per DRG No R0_9160/018.  The rate to include cutting and welding or jointing with flanges as required and for coating and lining as per specifications.  Flanges according to Rand Water specification (DRG No. A11791)"]
[]
[null,null,"REFER TO TABLE 1"]
[]
["14.12.2.1",null,"1450mm OD compensation plate, 16mm thick (1)","No.",6]
[]
["14.12.2.2",null,"610mm OD straight pipe, 9.5mm thick, flanged on one ends (2)","No.",6]
[]
["14.12.2.3",null,"323.8mm OD straight riser pipe, 9.52mm thick, flanged on both ends (3)","No.",6]
[]
["14.12.2.4",null,"DN300 gate valve flanged on both ends (4)","No.",6]
[]
["14.12.2.5",null,"DN300 Air valve (5)","No.",6]
[]
[null,null,"REFER TO TABLE 2"]
[]
["14.12.2.6",null,"1200mm OD compensation plate, 10mm thick (1)","No.",18]
[]
["14.12.2.7",null,"816mm OD straight pipe, 8mm thick, flanged on one ends (2)","No.",18]
[]
["14.12.2.8",null,"323.8mm OD straight riser pipe, 9.52mm thick, flanged on both ends (3)","No.",18]
[]
["14.12.2.9",null,"DN300 gate valve flanged on both ends (4)","No.",18]
[]
["14.12.2.10",null,"DN300 Air valve (5)","No.",18]
[]
[]
[null,null,"REFER TO TABLE 3"]
[]
["14.12.2.11",null,"1480mm OD compensation plate, 25mm thick (1)","No.",13]
[]
["14.12.2.12",null,"1020mm OD straight pipe, 9.52mm thick, flanged on one ends (2)","No.",13]
[]
["14.12.2.13",null,"323.8mm OD straight riser pipe, 9.52mm thick, flanged on both ends (3)","No.",13]
[]
["14.12.2.14",null,"DN300 gate valve flanged on both ends (4)","No.",13]
[]
["14.12.2.15",null,"DN300 Air valve (5)","No.",13]
["Total brought forward "]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate"]
["Total Carried Forward  "]
[]
["14.12.2.16",null,"8mm wrapper plate on B11 stiffened pipeline","No.",13]
[]
[]
[14.13,null,"CATHODIC INSULATING FLANGES"]
[]
[null,null,"Supply of flanges at cathodic insulating flanges for the following diameters, , including installation, fitting, tightening and setting of gasket rings, flange bolts, nuts and washers:"]
[]
["14.13.1",null,"a)  1800mm diameter (3500KPa)","No.",8]
[]
["14.13.2",null,"b)  2500mm diameter (3500KPa)","No.",2]
[]
[]
[14.14,null,"PUDDLE FLANGES"]
[]
[null,null,"Supply of puddle flanges at the chamber walls for the following diameters, , including installation and welding:"]
[]
["14.14.1",null,"a)  16mm, 150mm wide puddle flange for 1424mm diameter pipe","No ",3]
[]
["14.14.2",null,"a)  16mm thick, 150mm wide puddle flange for 1832mm diameter pipe","No ",11]
[]
["14.14.3",null,"a)  20mm thick, 200mm wide puddle flange for 2036mm diameter pipe","No.",6]
[]
["14.14.4",null,"a)  20mm thick, 200mm wide puddle flange for 2524mm diameter pipe","No.",2]
[]
[]
["Section 14 -  Carried Forward to Summary"]

{"sheet":"15.Pipeline - Pipeline Sundries","index":15,"n_rows":45,"n_cols":7,"rows_kept":45,"merged":[[2,9,2,11],[44,0,45,5],[44,6,45,6]],"flags":["formulas_cached_only"]}
[null,null,"Lethabo Pump Station: ",{"$nulls":3},"Section 15: Pressure Sundries"]
[null,null,"Header upgrade at Lethabo Pumping Station"]
[]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No","Refers"]
[]
[null,null,"SECTION 15:  PIPELINE SUNDRIES"]
[]
[15.1,"SABS 1200 DK","Gabions and Pitching"]
[]
["15.1.1","8.2.1 (a)","Surface preparation for bedding of gabions - cavities filled with excavated material or rock","m2",50]
[]
[null,null,"Supply and lay the following:"]
[]
["15.1.2","8.2.2","Gabions: "]
[]
["15.1.2.1",null,"2 x 1 x 1m boxes with rock","m3",20]
[]
["15.1.2.2",null,"3 x 1  0.3m mattress with rock","m3",10]
[]
["15.1.3","8.2.4","Geotextile (Bidim A7 or similar)","m²",50]
[]
["15.1.4","8.2.5","Supply and construct ordinary stone pitching including preparation and compacting of foundation, placing of 150mm nominal size stones in a 300mm thick grouting layer.","m2",50]
[]
[15.2,null,"Temporary Fences and Gates"]
[]
["15.2.1",null,"Supply, installation and removal of new fencing and gates including allowances for support posts at 3m intervals, straining posts and stays."]
[]
["15.2.1.1",null,"a) Diamond mesh wire security fencing up to 1.8m high","m",100]
[]
["15.2.1.2",null,"b)  Install 5m wide x 1,8m double gate","No",2]
{"$rows_empty":13}
["Section 15 Carried Forward to Summary"]

{"sheet":"16.Pipeline-Cathodic Protect","index":16,"n_rows":179,"n_cols":7,"rows_kept":179,"merged":[[42,0,42,5],[44,0,44,5],[88,0,88,5],[90,0,90,5],[139,0,139,5],[141,0,141,5],[165,0,166,5],[165,6,166,6]],"flags":["formulas_cached_only"]}
[null,null,"Lethabo Pump Station: ",{"$nulls":3},"Section 16: Cathodic Protection"]
[null,null,"Header upgrade at Lethabo Pumping Station"]
[]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No","Refers"]
[]
[]
[100,null,"SACP Installation Works: Sacrificial Anode Cathodic Protection"]
[101,null,"Supply and install Concrete Bunker as per RW TS003","ea",2]
[102,null,"Supply and Install 10kg HP Mg anodes bagged\nin Gypsom/Bentonite complete with 10mm2 tails as per TS055 incl. earthworks","ea",66]
[103,null,"Supply and Install Valve Chamber Test Point as per TS012","ea",12]
[104,null,"Supply and Install Cable to pipe connection including 200mm x 200mm coating repair. (as per TS015) ","ea",66]
[105,null,"Supply and Install  PRE and coupon  (as per TS004)","ea",14]
[106,null,"Supply and Install 16mm2 cabling  ","ea",200]
[107,null,"Excavation ,trenching and Backfilling for Cable Installation (RA 25785)  (as per TS019)","m",200]
[108,null,"Install link panel","ea",14]
[109,null,"Marker Plate ( 85x40x3)","ea",2]
[110,null,"Ø40mm x 2000mm Conduit Heavy  HDPE","ea",2]
[]
[200,null,"CP Installation Works: ICCP System"]
[201,null,"Supply and Install Transformer Rectifier unit - 3ph 100V/100A RW ELS 001","ea",1]
[202,null,"Supply and Install vandal proof Durasafe Enclosure with RMU and alarm (to incorporate infrared motion/vicinity sensors, seismic/shock sensors, magnetic contact sensors as a minimum) - RW ELS 001/Drawing","ea",1]
[203,null,"GROUNDING BUS BAR 400x50x5, TINNED COPPER","ea",1]
[204,null,"EARTHING ROD Ø16x4000 LONG, COPPER PLATED STEEL","ea",8]
[205,null,"HEX. BOLT M12x30 LONG C/W NUT,FLAT + SPRING WASHER, STAINLESS STEEL","ea",2]
[206,null,"HEX. BOLT M10x25 LONG C/W NUT,FLAT + SPRING WASHER, STAINLESS STEEL","ea",10]
[207,null,"CABLE LUG (M10X70mm2 CABLE), TINNED COPPER","ea",2]
[208,null,"SLEEVE WITH CAP (Ø110mm), PVC","ea",8]
[209,null,"1CORE MULTI STRAND 70mm2 600V CU CABLE PVC","m",60]
[210,null,"1CORE MULTI STRAND 70mm2 600V CU CABLE bare","m",12]
[211,null,"Install Earthing System","sum",1]
[212,null,"Grounding Rail","ea",1]
[213,null,"Electrical Isolation Switch Box","ea",1]
[214,null,"MMO Titanium Canisterized Anodes 200mm dia X 2000mm","ea",10]
[215,null,"Supply 2000mm length x 200mm diameter x 1mm thick galvanized steel canister spacer filled with calcined petroleum coke,","ea",10]
[216,null,"Supply and Install Cable to pipe connection including coating repair","ea",4]
[217,null,"Supply and install  PRE and coupon","ea",1]
[218,null,"Trenching and Backfilling for Cable Installation (RA 25785)","m2","As reqd."]
[219,null,"Excavation for GB (Groundbed trench 0,5x2,5m) and pipe to cable (Pipe cable trench 0,3x1m) installations ","m3","As reqd."]
[220,null,"Cable warning tape","m",1100]
[221,null,"Cable Tee Joint, epoxy (splicing kit)","ea",12]
[222,null,"Anode Main Ring 4core 35mm2 multi strand CU red cable PVC/PVC","m",1100]
["Total brought forward "]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate"]
["Total Carried Forward  "]
[223,null,"Supply and install  anode cable 1 core 35mm2 multi strand CU red cable PVC/PVC","m",1100]
[224,null,"Supply and install Cathode Cable: 1 core 35mm2 multi strand CU black cable PVC/PVC","m",100]
[225,null,"Supply and install Monitoring Cable 16mm2 multi starnd CU black cable PVC/PVC","m",100]
[226,null,"Supply and install PRE with a tail cable of 16mm2 multi starnd CU red cable PVC/PVC with a length of 100m","ea",1]
[227,null,"Supply and install Coupon with a tail cable of 16mm2 multi starnd CU black cable PVC/PVC with a length of 100m","ea",1]
[228,null,"Supply and install  16mm2 4CORE Cu armoured cable for AC supply","m",100]
[]
[230,null,"Crossbonding across the actuated valves and magflow meters"]
[null,null,"Phase 1"]
[231,null,"Supply and install steel conduit (6m per chamber) and saddles","sum",4]
[232,null,"Supply and install link panels","sum",3]
[233,"TS021","Supply 16mm² pipe cable for cross bonding","m",34]
[234,null,"Crossbonds across the actuator valves in a chamber","ea",3]
[235,null,"Crossbond across the magflow meter in a chamber  (no link panel)","ea",1]
[]
[null,null,"Phase 1B"]
[236,null,"Supply and install steel conduit (6m per chamber) and saddles","sum",2]
[237,null,"Supply and install link panels","sum",1]
[238,"TS021","Supply 16mm² pipe cable for cross bonding","m",18]
[239,null,"Crossbonds across the actuator valves in a chamber","ea",1]
[240,null,"Crossbond across the magflow meter in a chamber  (no link panel)","ea",1]
[]
[null,null,"Phase 2"]
[241,null,"Supply and install steel conduit and saddles","sum",2]
[242,null,"Supply and install link panels","sum",1]
[243,"TS021","Supply 16mm² pipe cable for cross bonding","m",18]
[244,null,"Crossbonds across the actuator valves in a chamber","ea",1]
[245,null,"Crossbond across the magflow meter in a chamber  (no link panel)","ea",1]
[]
[null,null,"Phase 3"]
[246,null,"Supply and install steel conduit and saddles","sum",2]
[247,null,"Supply and install link panels","sum",1]
[248,"TS021","Supply 16mm² pipe cable for cross bonding","m",18]
[249,null,"Crossbonds across the actuator valves in a chamber","ea",1]
[250,null,"Crossbond across the magflow meter in a chamber  (no link panel)","ea",1]
[]
[null,null,"Phase 4"]
[251,null,"Supply and install steel conduit and saddles","sum",2]
[252,null,"Supply and install link panels","sum",1]
[253,"TS021","Supply 16mm² pipe cable for cross bonding","m",18]
[254,null,"Crossbonds across the actuator valves in a chamber","ea",1]
[255,null,"Crossbond across the magflow meter in a chamber  (no link panel)","ea",1]
[]
["Total brought forward "]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate"]
["Total Carried Forward  "]
[]
[260,null,"IF Kits as per annexure 1"]
[null,null,"Phase 1"]
[261,"TS034","Supply and install full Insulation Flange Kit  1800mm diameter, on both side of the electromagnetic meter as per drawing No A_9548 Rev 2.","ea",2]
[262,"TS034","Supply and install full Insulation Flange (IF)  Kits on both side of the actuator valve diameter 1800mm, as per drawing No A_9548 Rev 2.","ea",2]
[263,"TS034","Supply and install full Insulation Flange Kits on both side of the actuator valve diameter 2000mm, as per drawing No A_9548 Rev 2.","ea",6]
[264,"TS034","Supply and install full Insulation Flange (IF)  Kits on both side of the actuator valve diameter 800mm, as per drawing No A_9548 Rev 2.","ea",4]
[265,null,"Supply and install a spark gaps or surge arrestors with the connecting plates (two plates per surge arrestor) across the actuated valves and the magflow meter.","ea",7]
[]
[null,null,"Phase 1B"]
[266,"TS034","Supply and install full Insulation Flange Kits  2500mm diameter, on both side of the electromagnetic meter as per drawing No A_9548 Rev 2.","ea",2]
[267,"TS034","Supply and Install full Insulation Flange (IF) Kits on both side of the actuator valve diameter 1800mm, as per drawing No A_9548 Rev 2.","ea",2]
[268,null,"Supply and install a spark gaps or surge arrestor with the connecting plates (two plates per surge arrestor) across the actuated valves and the magflow meter.","ea",2]
[]
[null,null,"Phase 2"]
[269,"TS034","Supply and install full Insulation Flange Kits  1800mm diameter, on both side of the electromagnetic meter as per drawing No A_9548 Rev 2.","ea",2]
[270,"TS034","Supply and install full Insulation Flange Kits on both side of the actuator valve diameter 1800mm, as per drawing No A_9548 Rev 2.","ea",2]
[271,null,"Supply and install a spark gaps or surge arrestors with the connecting plates (two plates per surge arrestor) across the actuated valves and the magflow meter.",null,2]
[]
[null,null,"Phase 3"]
[272,"TS034","Supply and install full Insulation Flange Kit  180mm diameter, on both side of the electromagnetic meter as per drawing No A_9548 Rev 2.","ea",2]
[273,"TS034","Supply and install full Insulation Flange Kit on both side of the actuator valve diameter 1800mm, as per drawing No A_9548 Rev 2.","ea",4]
[274,null,"Supply and install a spark gaps or surge arrestors with the connecting plates (two plates per surge arrestor) across the actuated valves and the magflow meter.","ea",3]
[]
[null,null,"Phase 4"]
[275,"TS034","Supply and install full Insulation Flange Kits  1800mm diameter, on both side of the electromagnetic meter as per drawing No A_9548 Rev 2.","ea",2]
[276,"TS034","Supply and install full Insulation Flange Kits on both side of the actuator valve diameter 1800mm, as per drawing No A_9548 Rev 2.","ea",2]
[277,null,"Supply and install a spark gaps or surge arrestors with the connecting plates (two plates per surge arrestor) across the actuated valves and the magflow meter.","ea",2]
[]
[280,null,"Marker becon","ea",6]
[]
[300,null,"CP Installation Works: Cross Bonding to Existing ICCP protected pipe"]
[301,null,"Interference Testing, Installation and cable termination of cross bond bunker  incl. termination , coupon + ref electrode, pipe to cable exothermic weld connection","ea",2]
[302,null,"Interference Testing, Installation and cable termination of cross bond bunker  incl. termination , coupon + ref electrode, pipe to cable exothermic weld connection","ea",3]
[303,null,"Interference Testing, Installation and cable termination of cross bond bunker  incl. termination , coupon + ref electrode, pipe to cable exothermic weld connection","ea",4]
[401,null,"Coating Removal and Rehabilitation","m2","As reqd."]
[402,null,"PCM Underground Services Detection (Steel Pipes Only)","km","As reqd."]
[403,null,"Ground Penetrating Radar Services Detection (Electrical Cables, Plastcic/Steel Piping etc.)","km","As reqd."]
[]
[500,null,"Commissioning and Testing"]
[501,null,"Post Installation 24Hr Interference Potential Tests","sum",1]
[502,null,"Final Documentation and Handover","sum",1]
[]
[600,null,"AC Mitigation: Supply and Delivery at Valve Chambers"]
[601,null,"Voltage Limiting Device with IP68 enclosure and DIN rail to RW spec CPS 1.45, drwg. RA_27373 (See Note 1) (1 per valve chamber, 2 per flow meter chamber)","ea",23]
[602,null,"Dairyland PCR-3.5KA/80A-S-CS2 or equiv. for Sasol / Eskom IFs (see Note 2)","ea",7]
[603,null,"Steel weld mesh 200 x 200 mm, 6 mm Ø, not galvanized","m2",9]
[]
["Total brought forward "]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate"]
["Total Carried Forward  "]
[604,null,"Re-bar connecting plate, stainless steel, to drawing RA_27375, but with 12 mm Ø hole (1 per valve chamber, 2 per flow meter chamber)","ea",23]
[605,null,"Screed mix for weld mesh encapsulation","m3","0.5"]
[606,null,"Multistrand 16mm2 Cu cable PVC/PVC yellow/green for weld mesh or re-bar connection (4m per valve chamber, 8m per flow meter chamber)","m",92]
[607,null,"Multistrand 16mm2 Cu cable PVC/PVC black for pipeline connection","m",92]
[608,null,"Pin brazing material and M10 stud bolt for pipeline connection (1 per valve chamber, 2 per flow meter chamber)","ea",23]
[609,null,"Thermit or arc welding material for connecting re-bar in new valve chambers (number of welds required will depend on re-bar density and chamber size)","chambers",17]
[610,null,"Cable lugs for 16 mm2 cable for M10 and connector plate connection (4 per valve chamber, 8 per flow meter chamber)","ea",92]
[611,null,"Fasteners for VLD enclosure and DIN rail","set",23]
[612,null,"M10 bolt, screw and washers for connecting cable lug to connector plate","set",23]
[613,null,"Squish pack Hi-Cote 151E epoxy coating for pipeline and connector plate connections (1 per valve chamber, 2 per flow meter chamber)","ea",23]
[614,null,"Cable saddles for weld mesh fitment","packet",1]
[]
[700,null,"AC Mitigation: Installation at Valve Chambers"]
[701,null,"New chamber: Weld Re-bar at all intersections of two (2) diagonal bars in chamber floor and all uprights at continuity ring in chamber walls (see Note)","ea",17]
[702,null,"New chamber: Weld Re-bar connecting plate to continuity ring prior to casting (1 per valve chamber, 2 per flow meter chamber)","ea",21]
[703,null,"Existing chamber: Fully cover floor with weld mesh cut-out and pin down with cable saddles","ea",1]
[704,null,"Existing chamber: Weld connecting plate to weld mesh (1 per valve chamber, 2 per flow meter chamber)","ea",2]
[705,null,"Existing chamber: Pour layer of screed (3 cm nom.) over weld mesh and level off ensuring proper drainage","ea",1]
[706,null,"Pipe connection: Locally remove pipeline coating, pin braze M10 stud onto pipe and apply epoxy coating over weld area (ref. CPS 1.34) (1 per valve chamber, 2 per flow meter chamber)","ea",23]
[707,null,"Crimp cable lugs to cable ends (one side only) (4 per valve chamber, 8 per flow meter chamber)","ea",92]
[708,null,"Install Voltage Limiting Device in chamber and connect all wiring with double connections (1 per valve chamber, 2 per flow meter chamber) NB Cables kept as short as possible","ea",23]
[709,null,"Encapsulate cable lug connections with epoxy coating","ea",46]
[710,null,"Install PCR device across existing Eskom/Sasol IFs at the pump outlets and at chambers 6 & 7.","ea",7]
["Section 16 Carried Forward to Summary"]
[]
[null,"Notes and Assumptions"]
[]
[null,"Note 1: Locally available product. Dairyland SSD-2/2-1.2-75 is also suitable "]
[null,"Note 2: Locally available VLDs to RW spec CPS 1.45 is also suitable for IFs"]
[]
[null,"Valve chambers: 8 new (ch 3, 4, 5, 6, 7, 8,12,13)"]
[null,"Flow meter chambers : 4 new (ch 2A, 2B, 11, 15) and 1 existing (ch 9)"]
[null,"Air valve chambers: 5 new"]
[null,"Eskom/Sasol IFs: 5 existing, 2 new (ch 6 & 7)"]
[null,"All new chambers must still be constructed (if already built, use weld mesh method in lieu of re-bar method and "]
[null,"adapt quantities accordingly)"]
[null,"Existing Eskom and Sasol chambers must still be added (yellow highlight items) number of chambers TBC"]

{"sheet":"17. Mechanical Header","index":17,"n_rows":206,"n_cols":7,"rows_kept":206,"merged":[[40,0,40,5],[42,0,42,5],[82,0,82,5],[84,0,84,5],[124,0,124,5],[126,0,126,5],[160,0,160,5],[162,0,162,5],[205,0,206,5],[205,6,206,6]],"flags":["formulas_cached_only"]}
[]
[null,null,"Lethabo Pump Station: ",null,null,"Section 17: Mechanical "]
[null,null,"Header upgrade at Lethabo Pumping Station"]
["Item No.","Reference:  RW10396363/21/Mech-Spec","Description","UOM","QTY","Rate ","Amount "]
[17,null,"SECTION 17:  MECHANICAL"]
[17.1,null,"PHASE ONE (1) "]
[]
["17.1.1",2.5,"BUTTERFLY VALVES:"]
[null,null," Remove, refurbish and test valves as per Rand Water SpecifictionRW-12/1/4/-AS 0925. Deliver to Rand Water Central Depot  "]
[]
["17.1.1.1",null,"2000mm dia ","No",2]
[]
["17.1.1.2",null,"800mm","No",2]
[]
["17.1.1.3",null,"200mm dia - by pass  excluding actuator ","Sum",1]
[]
["17.1.2",2.1,"Manufacture, Test, Supply and delivey of  flanged isolating butterfly valves, including dismantling couplings and gaskets. Flanged to A11791 5 000KPa Test Pressure complying to Rand Water specifications. RW /0310/AS 0460"]
[]
["17.1.2.1",null,"2000mm dia","No",3]
[]
["17.1.2.2",null,"1800mm dia","No",2]
[]
["17.1.2.3",null,"800 mm dia",null,2]
[]
["17.1.3",2.4,"Manufacture, Test, Supply and delivey of  flanged Surge Anticpation Valve","No",2]
[]
["17.1.4",2.1,"Manufacture, Test, Supply and delivery of actuator, complete with gearbox, actuator extension and fittings etc. for butterfly valve with TP  5 000 kPa valve: "]
[]
["17.1.4.1",null,"2000mm dia","No",3]
[null,null," "]
["17.1.4.2",null,"1800mm dia","No",2]
[]
["17.1.4.3",null,"800 mm dia","No",2]
[]
["17.1.5",2.2,"NON RETURN VALVES"]
[null,null,"Manufacture, Test, Supply and delivery of NRV  valve as per Rand Water Specifiction RW/0310/AS0460  delivery of a flanged non return valve, including dismantling couplings and gaskets. Flanged to A11791, 5 000kPa Test Pressure complying to Rand Water specifications."]
[]
["17.1.5.1",null,"1400mm dia","No",2]
[]
["17.1.6",2.4,"Manufacture, Test, Supply and delivey of  flanged Surge Anticpation Valve","No",2]
["Total brought forward "]
["Item No.","Reference:  RW10396363/21/Mech-Spec","Description","UOM","QTY","Rate ","Amount "]
["Total Carried Forward  "]
[]
["17.1.7",2.3,"AIR VALVES"]
[null,null,"Manufacture, Test, Supply and delivey of  Air valve complete with isolating gate valve and  fittings etc, complying with SANS 664 and have   5 000 KPa Test Pressure."]
[]
["17.1.7.1",null,"a) 300mm dia","No",3]
[]
["17.1.8",null,"Installation, commissioning and putting into service of valves complete  with  actuator, gaskets , fitttings bolts and nuts etc. ","Sum","Sum"]
[]
["17.1.9",2.6,"SUMP PUMPS"]
[null,null,"Supply and deliver sump sumps complete with impellor, motor, strainer, fittings  and delivery steel connecting to the 450 mm scour pipe as shown on drawing R0 9160/100 and R09160/101. Submersible sump pump unit    complete with Non return valve, Isolation valve, pump delivery pipe, fittings hold down U- bolts and drain pipe  for  Chamber: "]
[]
["17.1.9.1",null,"Chamber 2A","Sum",1]
[]
["171.9.2",null,"Chamber 3","Sum",1]
[]
["17.1.9.3",null,"Chamber 4","Sum",1]
[]
["17.1.9.4",null,"Chamber 6","Sum",1]
[]
["17.1.9.5",null,"Chamber 7","Sum",1]
[]
["17.1.9.6",null,"Chamber 8","Sum",1]
[]
["17.1.9.7",null,"Chamber 9","Sum",1]
[]
["17.9.8",null,"Isolation Valve","No",7]
[]
["17.1.9.9",null,"Non Return Valve ","No",7]
[]
[17.2,null,"PHASE TWO (2) "]
[]
["17.2.1",2.1,"BUTTERFLY VALVES:"]
[null,null,"Manufacture, Test, Supply and delivey of  flanged isolating butterfly valves, including dismantling couplings and gaskets. Flanged to A11791 5 000KPa Test Pressure complying to Rand Water specifications. RW /0310/AS 0460"]
[]
["17.2.1.1",null,"1800mm dia","No",1]
[]
["17.2.1.2",2.1,"Manufacture, Test, Supply and delivery of actuator, complete with gearbox, actuator extension and fittings etc. for butterfly valve with TP  5 000 kPa valve: "]
[]
[null,null,"1800mm dia",null,1]
["Total brought forward "]
["Item No.","Reference:  RW10396363/21/Mech-Spec","Description","UOM","QTY","Rate ","Amount "]
["Total Carried Forward  "]
[]
["17.2.2",2.2,"NON RETURN VALVES"]
[null,null,"Manufacture, Test, Supply and delivery of NRV  valve as per Rand Water Specifiction RW/0310/AS0460  delivery of a flanged non return valve, including dismantling couplings and gaskets. Flanged to A11791, 5 000kPa Test Pressure complying to Rand Water specifications."]
[]
["2.2.2.1",null,"1400mm dia","No",1]
[]
["17.2.3",2.4,"Manufacture, Test, Supply and delivey of  flanged Surge Anticpation Valve","No",1]
[]
["17.2.4",2.3,"AIR VALVES"]
[null,null,"Manufacture, Test, Supply and delivey of  Air valve complete with isolating gate valve and  fittings etc, complying with SANS 664 and have   5 000 KPa Test Pressure."]
[]
["17.2.4.1",null,"a) 400mm dia","No",1]
[]
["17.2.5",null,"Installation, commissioning and putting into service of valves complete  with  actuator, gaskets , fitttings bolts and nuts etc. ","Sum ",1]
[]
["17.2.6",2.6,"SUMP PUMPS"]
[null,null,"Supply and deliver sump sumps complete with impellor, motor, strainer, fittings  and delivery steel connecting to the 450 mm scour pipe as shown on drawing R0 9160/100 and R09160/101. Submersible sump pump unit    complete with Non return valve, Isolation valve, pump delivery pipe, fittings hold down U- bolts and drain pipe  for  Chamber: "]
[]
["17.2.6.1",null,"Chamber 2B","Sum",1]
[]
["17.2.6.2",null,"Isolation Valve","No",1]
[]
["17.2.6.3",null,"Non Return Valve ","No",1]
[]
[17.3,null,"PHASE THREE (3) "]
[]
["17.3.1",2.1,"BUTTERFLY VALVES"]
[null,null,"Manufacture, Test, Supply and delivey of  flanged isolating butterfly valves, including dismantling couplings and gaskets. Flanged to A11791 5 000KPa Test Pressure complying to Rand Water specifications. RW /0310/AS 0460"]
[]
["17.3.1.1",null,"2000mm dia","No",1]
[]
["17.3.1.2",null,"1800mm dia","No",2]
[]
["17.3.2",2.1,"Manufacture, Test, Supply and delivery of actuator, complete with gearbox, actuator extension and fittings etc. for butterfly valve with TP  5 000 kPa valve: "]
[]
["17.3.2.1",null,"2000mm dia","No",1]
[null,null," "]
["17.3.2.2",null,"1800mm dia","No",2]
[]
["Total brought forward "]
["Item No.","Reference:  RW10396363/21/Mech-Spec","Description","UOM","QTY","Rate ","Amount "]
["Total Carried Forward  "]
[]
["17.3.3",2.2,"NON RETURN VALVES"]
[]
[null,null,"Manufacture, Test, Supply and delivey of  Air valve complete with isolating gate valves and  fittings etc, complying with SANS 664 and have   5 000 KPa Test Pressure."]
[]
["17.3.3.1",null,"1400mm dia","No",2]
[]
[]
["17.3.4",2.4,"Manufacture, Test, Supply and delivey of  flanged Surge Anticpation Valve","No",2]
[]
["17.3.5",null,"AIR VALVES"]
[null,2.3,"Manufacture, Test, Supply and delivey of  Air valve complete with isolating gate valve and  fittings etc, complying with SANS 664 and have   5 000 KPa Test Pressure."]
[]
["17.3.5.1",null,"a) 300mm dia","No",2]
[]
["17.3.6",null,"Installation, commissioning and putting into service of valves complete  with  actuator, gaskets , fitttings bolts and nuts etc. "]
[]
["17.3.7",2.6,"SUMP PUMPS"]
[null,null,"Supply and deliver sump sumps complete with impellor, motor, strainer, fittings  and delivery steel connecting to the 450 mm scour pipe as shown on drawing R0 9160/100 and R09160/101. Submersible sump pump unit    complete with Non return valve, Isolation valve, pump delivery pipe, fittings hold down U- bolts and drain pipe  for  Chamber: "]
["17.3.7.1",null,"Chamber 5","Sum",1]
[]
["17.3.7.2",null,"Chamber 11","Sum",1]
[]
["17.3.7.3",null,"Chamber 12","Sum",1]
[]
["17.3.7.4",null,"Chamber 13","Sum",1]
[]
["17.3.7.5",null,"Chamber 14","Sum",1]
[]
["17.3.7.6",null,"Isolation Valve","No",5]
[]
["17.3.7.7",null,"Non Return Valve ","No",5]
[]
["Total brought forward "]
["Item No.","Reference:  RW10396363/21/Mech-Spec","Description","UOM","QTY","Rate ","Amount "]
["Total Carried Forward  "]
[17.4,null,"PHASE FOUR (4) "]
[]
["17.4.1",2.6,"SUMP PUMPS"]
[null,null,"Supply and deliver sump sumps complete with impellor, motor, strainer, fittings  and delivery steel connecting to the 450 mm scour pipe as shown on drawing R0 9160/100 and R09160/101. Submersible sump pump unit    complete with Non return valve, Isolation valve, pump delivery pipe, fittings hold down U- bolts and drain pipe  for  Chamber: "]
[]
["17.4.1.1",null,"Chamber 15","Sum",1]
[]
["17.4.1.2",null,"Isolation Valve","No",1]
[]
["17.4.1.3",null,"Non Return Valve ","No",1]
[]
["17.4.2",null,"Installation, commissioning and putting into service of sump  pumps complete  with  Valves, NRVs, piping and fittings etc.  ","Sum",1]
[]
[17.5,2.7,"Surge Tank "]
[null,null,"Dismentle existing Surge Tank and remove pipes and valves and fttings  ","Sum",1]
["17.5.1"]
["17.5.2",null,"Design and construct foundation for the  tank, chambers, valves and associated pipes etc. (new location for the surge tank & associated equipement)  ","Sum",1]
[]
[]
[]
["17.5.3",2.7,"Existing Surge Tank "]
[]
["17.5.3.1",null,"Assess and check the adequacy of the design for the existing surge tank","Sum",1]
[]
["17.5.3.1.1",null,"Tank Refurbishment   "]
[]
["17.5.3.1.1.1","2.7.1& 2.7.2","Remove, tranport,refurbish, deliver, relocate and re-install a 315 kL  Steel Water hammer tank complete with valves, piping and fitting etc.      ","Sum",1,null,"Rate Only "]
[]
["17.5.3.1.1.2",null,"Manufacture , supply & Deliver new valves coplete with fittings for the surge tanks ","Sum",1,null,"Rate Only "]
[]
[]
[17.6,null,"Operation & Maintenance Manuals  (six copies)","Sum",1]
[]
[]
[17.7,null,"Maintenance during the defects & liability period.","Sum",1]
[]
[17.8,null,"All other equipment /consumables/service  not stated above which are  required to complete and commission the Installation"]
[]
[18,null,"Refurbishment of Pump Set Magflow Meters- Collection , transport , refurbiment and installation of Pump Set Magflow Meters "]
["18..1",null,"diameter 1800mm ","No",4]
[]
[]
["Section 17 Carried Forward to Summary"]

{"sheet":"18. Mechanical Refurb","index":18,"n_rows":64,"n_cols":7,"rows_kept":64,"merged":[[0,3,0,6],[63,0,64,5],[63,6,64,6]],"flags":["formulas_cached_only"]}
[null,null,"Lethabo Pump Station: ","Section 18: Pumps & Rotaty Screen "]
[null,null,"Header upgrade at Lethabo Pumping Station"]
["Item No.","Reference:RW10396363/21/Pump-Refurb/Spec","Description","UOM","QTY","Rate ","Amount "]
["18",null,"SECTION 18 : MECHANICAL - MANUFACTURE SUPPLY, DELIVERY, INSTALLATION & COMMISSIONING "]
[]
[]
[18.1,null,"Manufacture, test,  supply, and delivery"]
[]
["18.1.1",3.3,"Suction and Delivery Pipework"]
["18.1.1.1",null,"Manufacture, supply and delivery of suction and delivery pipework, all fittings, specials, and pipe supports as typical shown on drawing RA 39618. & 9398","Set ",4]
[]
["18.1.2",3.4,"Suction and Delivery valves"]
["18.1.2.1",null,"Manufacture, supply and delivery of electrically operated TP   5 000 kPa suction butterfly valve and TP 5 000 kPa delivery butterfly check valve.","Each",8]
[]
["18.1.3",3.5,"Rotary screen refurbishment and replacement work"]
[null,null,"The contractor shall be required to determine the condition of the rotary screens and modify, refurbish/ replace componets as detailed in the mechanical scope of work. The work to be complete shall comprise of but not limited to the following:"]
["18.1.3.1",null,"Removal and stripping of rotary screen units","Each",4]
["18.1.3.2",null,"Sand Blasting of Rotary Screen Components","Each",4]
["18.1.3.3",null,"Rotary Screen Refurbishment & Cleaning ","Each",4]
["18.1.3.4",null,"Inspection of complete refurbishment","Each",4]
["18.1.3.5",null,"Coating of the Rotary Screen Components","Each",4]
["18.1.3.6",null,"Replacement of Rotary Screen Components (screen panels, tension sprocket )","Each",4]
["18.1.3.7",null,"Drive system: 3  kW IP68   rated enclosure  motors complete with cabling, fittings, glands and stop start switch etc.\nDrive gear box complete with fittings. ","Each",4]
["18.1.3.8",null,"Manufacture, supply and delivery of main bearings","Each",8]
["18.1.3.9",null,"Modification of coarse screen gates","Each",4]
["18.1.3.10",null,"Manufacture, supply and delivery of access steel work","Sum",1]
["18.1.3.11",null,"Manufacture, supply and delivery of spray water pipe system. Refer to drawing M10245.","Sum",1]
[]
["18.1.4",3.6,"Rotating Element"]
[null,null,"Manufacture, test, supply, and delivery of a complete new set of rotating element for  450 Ml/d, 54 m double vlolute vertical pumps. \nThe rotating element shall comprise but not limited to the following:"]
["18.1.4.1",null,"Shaft","Each",1]
["18.1.4.2",null,"Impeller","Each",1]
["18.1.4.3",null,"Shaft sleeve DE & NDE","Each",2]
["18.1.4.4",null,"Sleeve nut DE & NDE","Each",2]
["18.1.4.5",null,"Stuffing box bush DE & NDE","Each",2]
["18.1.4.6",null,"Stuffing box bearing DE & NDE","Each",2]
["18.1.4.7",null,"Gland - split DE & NDE","Each",2]
["18.1.4.8",null,"Water thrower DE & NDE","Each",2]
["18.1.4.9",null,"Bearing assembly DE ","Each",1]
["18.1.4.10",null,"Bearing assembly NDE complete with double thrust bearing assembly ","Each",1]
["18.1.4.11",null,"Casing wear ring DE & NDE","Each",2]
[]
["1.8.1.5",3.7,"Pump Casing"]
["18.1.5.1",null,"Manufacture, supply and deliver a new pump casing for vertical split, double volute 450 Ml/d pump.","Each",1]
[]
[18.2,null,"Installation, commissioning and putting into service of Equipment  "]
[]
["18.2.1",3.3,"Suction and Delivery Pipework"]
["18.2.1.1",null,"Installation, commissioning and putting into service of suction and delivery pipework","Set",4]
[]
["18.2.2",3.4,"Suction and Delivery valves"]
["18.2.2.1",null,"Installation, commissioning and putting into service of actuated suction and delivery valves.","Set",4]
[]
["18.2.3",3.5,"Rotary screen refurbishment and replacement"]
["18.2.3.1",null,"Installation, commissioning and putting into service of refurbished rotary screen and associated system componets.","Set",4]
[]
[18.3,null,"Maintenance during the Defects and Liabilty Period","Sum",1]
[]
[18.4,null,"Training of Rand Water personnel. ","Sum",1]
[]
[18.5,null,"Preparation and submission of as built documentation including comprehensive operating and maintenance manuals","Sum",1]
[]
[18.6,null,"All other equipment /consumables/service  not stated above which are  required to complete and commission the Installation"]
["Section 18 Carried Forward to Summary"]

{"sheet":"19. Access Road ","index":19,"n_rows":1329,"n_cols":7,"rows_kept":1329,"merged":[[65,0,65,2],[131,0,131,2],[194,0,194,2],[261,0,261,2],[336,0,336,2],[402,0,402,2],[466,0,466,2],[524,0,524,2],[593,0,593,2],[661,0,661,2],[723,0,723,2],[795,0,795,2],[866,0,866,2],[934,0,934,2],[997,0,997,2],[1067,0,1067,2],[1138,0,1138,2],[1210,0,1210,2],[1281,0,1281,2],[1287,0,1287,6],[1328,1,1328,5]],"flags":["formulas_cached_only"]}
[null,null,"Lethabo Pump Station: ",{"$nulls":3},"Section 19: Access Road"]
[null,null,"Header Upgrade at Lethabo Pumping Station",null,null,"COLTO: ",1200]
[]
["Item No.","Payment Ref."," Description","Unit","Quantity","Rate","Amount R"]
[19.1,"1200"," GENERAL REQUIREMENTS AND PROVISIONS"]
[]
[]
[]
["19.1.1","B12.01","Provisional Sums for attendnce by the Design Engineer"]
[]
["19.1.1.1",null,"a) Level Site supervision","P.Sum",{"v":1,"d":" 1.0"},null,{"v":250000,"d":"250 000.0"}]
[]
["19.1.1.2",null,"(b) Design changes & As Built Drawings","P.Sum",{"v":1,"d":" 1.0"},null,{"v":150000,"d":"150 000.0"}]
[]
["19.1.1.3",null,"( c) Handling fees by the contractor","%",{"v":400000,"d":"400 000.0"}]
[]
["19.1.2","B12.02","Provisional Sums for additional testing"]
[]
["19.1.2.1",null,"(a) Geotechnical Investigations including Dynamic cone penetration as and when instructed by the Design Engineer","P. Sum",{"v":1,"d":" 1.0"},null,{"v":100000,"d":"100 000.0"}]
[]
["19.1.2.2",null,"(b) Identification of Services of surface and subsurface services on all roads to be worked on and submission of a complete services detection drawing and report to Rand water for acceptance (prior to construction)\n","P.Sum",{"v":1,"d":" 1.0"},null,{"v":100000,"d":"100 000.0"}]
[]
["19.1.2.3",null,"(c) Handling fee by the contractor","%",{"v":200000,"d":"200 000.0"}]
[]
["19.1.3","B12.03","Provisional Sum for the raising of manholes and re-using sme heavy duty covers","P. Sum",null,null,{"v":100000,"d":"100 000.0"}]
{"$rows_empty":40}
[" Total Carried Forward To Access Road Summary "]
[]
[]
[null,null,"Lethabo Pump Station: ",{"$nulls":3},"Section 19: Access Road"]
[null,null,"Header Upgrade at Lethabo Pumping Station",null,null,"COLTO: ",1300]
[]
["Item No.","Payment Ref."," Description","Unit","Quantity","Rate","Amount R"]
[18.2,1300," GENERAL REQUIREMENTS"]
[]
["18.2.1","B13.03","Identification, Protection, relocation, temporary stockpiling and reinstatement of existing services only where specifically instructed by the Engineer (Provisional) :","Prov sum",{"v":1,"d":" 1.0"},{"v":350000,"d":"350 000.00"},{"v":350000,"d":"350 000.00"}]
[]
["18.2.2","B13.04","Record Keeping and Progress Reporting"]
[]
["18.2.2.1",null,"a) Daily recording of site conditions, events and activities, including progress photographs","L/sum",{"v":1,"d":" 1.0"}]
[]
["18.2.2.2",null,"b) Collection of information as construction proceeds for as built record complilation at of contract completion","L/sum",{"v":1,"d":" 1.0"}]
[]
["18.2.2.3",null,"c) Production of as built drawings at completion of contract ","L/sum",{"v":1,"d":" 1.0"}]
[]
["18.2.3","B13.05","24 Hour Armed Mobile Security for the duration of the Contract","L/Sum",{"v":1,"d":" 1.0"}]
{"$rows_empty":46}
[" Total Carried Forward To Access Road Summary "]
[]
[null,null,"Lethabo Pump Station: ",{"$nulls":3},"Section 19: Access Road"]
[null,null,"Header Upgrade at Lethabo Pumping Station",null,null,"COLTO: ",1500]
[]
["Item No.","Payment Ref."," Description","Unit","Quantity","Rate","Amount R"]
[18.3,1500,"ACCOMODATION OF TRAFFIC"]
[]
["18.3.1",15.01,"Accomodation of traffic and maintaining temporary deviations:"]
[]
["18.3.1.2",null,"a) on the access route","km",{"v":1,"d":" 1.0"}]
[]
["18.3.1.3",null,"b) cut to spoil","m³",{"v":3,"d":" 3.0"}]
[]
["18.3.2","B15.03","Temporary traffic-control facilities: "]
[]
["18.3.2.1",null,"a) Flagmen","man-day",{"v":0,"d":" 0.0"}]
[]
["18.3.2.2",null,"b) Portable STOP and GO-RY signs","No",{"v":5,"d":" 5.0"}]
[]
["18.3.2.3",null,"d) Amber flicker lights","No",{"v":7,"d":" 7.0"}]
[]
["18.3.2.4",null,"e) Road signs, R- and TR-series, (1200mm)","No",{"v":5,"d":" 5.0"}]
[]
["18.3.2.5",null,"f) Road sign TW-series, (1200mm)","No",{"v":5,"d":" 5.0"}]
[]
["18.3.2.6",null,"g) Road signs, STW-DTG-TGS and TG-series (excluding delineators and barricades)","m²",{"v":3,"d":" 3.0"}]
[]
["18.3.2.7",null,"h) Delineators (TW402 + TW401) (200mm X 800mm)"]
[]
["18.3.2.7.1",null,"(i) Single","No",{"v":23,"d":" 23.0"}]
[]
["18.3.2.7.2",null,"(ii) Mounted back to back","No",{"v":35,"d":" 35.0"}]
[]
["18.3.2.7.3",null,"(j) Traffic cones (650mm high with fluorescent coating)","No",{"v":20,"d":" 20.0"}]
[]
["18.3.2.7.4",null,"(l) Movable barriers (portable New Jersey Barriers)","m",{"v":20,"d":" 20.0"}]
[]
["18.3.2.8",null,"(n) Provision of other traffic control measures ordered by the Engineer:"]
[]
["18.3.2.8.1",null,"(i) Provision of other traffic control measures","Prov sum",{"v":1,"d":" 1.0"},{"v":75000,"d":"75,000.00"},{"v":75000,"d":"75,000.00"}]
[]
["18.3.2.8.2",null,"(ii) Handling costs and profits in respect of sub-item B15.03(n)(i)","%"]
[]
["18.3.3",15.06,"Watering of temporary deviations","km",{"v":2,"d":" 2.0"}]
[]
["18.3.4",15.07,"Blading by road grader of "]
[]
["18.3.4.1",null,"(a) Existing roads used as temporary deviations","km-pass",{"v":5,"d":" 5.0"}]
[]
["18.3.5","B15.10","Accomodation of traffic where the road is constructed in half-widths as per standard drawings","km",{"v":1,"d":" 1.0"}]
[]
["18.3.6","B15.15","Provision of traffic safety equipment for use by the Engineer:"]
[]
["18.3.6.1",null,"(a) Amber flashing lights (firebeam orange 20300 or similar) with 2 No spare bulbs","No",{"v":4,"d":" 4.0"}]
[]
["18.3.6.2",null,"(b) Magnetic strip with words \"ROAD INSPECTION\" (100mm high lettering for use on vehicles)","No",{"v":4,"d":" 4.0"}]
[]
["18.3.6.3",null,"(c) High-visibilty safety jackets","No",{"v":8,"d":" 8.0"}]
[]
["18.3.7","B15.16","Traffic Safety Officer","month",6]
[]
[]
[" Total Carried Forward To Access Road Summary "]
[]
[null,null,"Lethabo Pump Station: ",{"$nulls":3},"Section 19: Access Road"]
[null,null,"Header Upgrade at Lethabo Pumping Station",null,null,"COLTO: ",1700]
[]
["Item No.","Payment Ref."," Description","Unit","Quantity","Rate","Amount R"]
[18.4,1700,"CLEARING AND GRUBBING"]
[]
["18.4.1","B17.01","Clearing and grubbing","ha",{"v":1.3750000000000002,"d":" 1.4"}]
[]
["18.4.2",17.02,"Removal and grubbing of large trees and tree stumps"]
[]
["18.4.2.1",null,"(b) Girth exceeding 1m up to and including 2m","No",{"v":5,"d":" 5.0"}]
[]
["18.4.2.2",null,"(a) Girth exceeding 2m up to and including 3m","No",{"v":2,"d":" 2.0"}]
[]
["18.4.3",17.04,"Clearing and grubbing at inlets and outlets of hydraulic structures","ha",{"v":0.2,"d":" 0.2"}]
[]
["18.4.4",17.06,"Removal and storage of selected vegetation "]
[]
["18.4.4.1",null,"(a) Cost of removal, storing, protection and replanting in a protected and fenced-off area of selected vegetation","Prov sum",{"v":1,"d":" 1.0"},{"v":75000,"d":"75,000.00"},{"v":75000,"d":"75,000.00"}]
[]
["18.4.4.2",null,"(b) Charge on provisional sum","%",{"v":75000,"d":"75,000.00"}]
[]
["18.4.5","B17.07","Removal of topsoil and temporary stockpilling thereof"]
[]
["18.4.5.1",null,"(a) Topsoil in temporary stockpiles","m³",{"v":2062.5,"d":"2 062.5"}]
[]
["18.4.6","B17.08","Relocation of:"]
[]
["18.4.6.1",null,"(a) Cathodic protection","Prov sum",{"v":1,"d":" 1.0"},{"v":100000,"d":"100,000.00"},{"v":100000,"d":"100,000.00"}]
[]
["18.4.6.2",null,"(b) Flow meter","Prov sum",{"v":1,"d":" 1.0"},{"v":120000,"d":"120,000.00"},{"v":120000,"d":"120,000.00"}]
[]
["18.4.6.3",null,"(c) Electrical pole","Prov sum",{"v":1,"d":" 1.0"},{"v":100000,"d":"100,000.00"},{"v":100000,"d":"100,000.00"}]
{"$rows_empty":32}
[" Total Carried Forward To Access Road Summary "]
[]
[null,null,"Lethabo Pump Station: ",{"$nulls":3},"Section 19: Access Road"]
[null,null,"Header Upgrade at Lethabo Pumping Station",null,null,"COLTO: ",1800]
[]
["Item No.","Payment Ref."," Description","Unit","Quantity","Rate","Amount R"]
[18.5,"B1800","DAYWORK"]
[]
["18.5.1","B18.01","Personnel","Prov sum",{"v":1,"d":" 1.0"},{"v":100000,"d":"100,000.00"},{"v":100000,"d":"100,000.00"}]
[]
[null,null,"(a) Unskilled labour","h",{"v":0,"d":"0.0"},null,"RATE ONLY"]
[]
[null,null,"(b) Semi-skilled labour","h",{"v":0,"d":"0.0"},null,"RATE ONLY"]
[]
[null,null,"(c) Skilled labour","h",{"v":0,"d":"0.0"},null,"RATE ONLY"]
[]
[null,null,"(d) Chargehand","h",{"v":0,"d":"0.0"},null,"RATE ONLY"]
[]
[null,null,"(e) Artisan","h",{"v":0,"d":"0.0"},null,"RATE ONLY"]
[]
[null,null,"(f) Foreman","h",{"v":0,"d":"0.0"},null,"RATE ONLY"]
[]
["18.5.2","B18.02","Equipment","Prov sum",{"v":1,"d":" 1.0"},{"v":500000,"d":"500,000.00"},{"v":500000,"d":"500,000.00"}]
[]
["18.5.2.1",null,"(a) CAT 926 (82KW) wheel loader","h",{"v":0,"d":"0.0"},null,"RATE ONLY"]
[]
["18.5.2.2",null,"(b) CAT 320 LME (96KW) crawler excavator","h",{"v":0,"d":"0.0"},null,"RATE ONLY"]
[]
["18.5.2.3",null,"(c) CAT 320 LME (96KW) crawler excavator","h",{"v":0,"d":"0.0"},null,"RATE ONLY"]
[]
["18.5.2.4",null,"(d) CAT 428 C (52KW) backhoe loader","h",{"v":0,"d":"0.0"},null,"RATE ONLY"]
[]
["18.5.2.5",null,"(e) CAT 140G grader","h",{"v":0,"d":"0.0"},null,"RATE ONLY"]
[]
["18.5.2.6",null,"(f) 10000-1400l water cart","h",{"v":0,"d":"0.0"},null,"RATE ONLY"]
[]
["18.5.2.7",null,"(g)Tip truck 10m3","h",{"v":0,"d":"0.0"},null,"RATE ONLY"]
[]
["18.5.2.8",null,"(h) Tip truck 6m3","h",{"v":0,"d":"0.0"},null,"RATE ONLY"]
[]
["18.5.2.9",null,"(i) Flat truck with 7t hydraulic crane","h",{"v":0,"d":"0.0"},null,"RATE ONLY"]
[]
["18.5.2.10",null,"(j) 5kW 12kg vibrating plate compactor","h",{"v":0,"d":"0.0"},null,"RATE ONLY"]
[]
["18.5.2.11",null,"(k) 23kW 1.8 tandem vibrating roller","h",{"v":0,"d":"0.0"},null,"RATE ONLY"]
[]
["18.5.2.12",null,"(l) 17t single drum self-propelled vibrating roller","h",{"v":0,"d":"0.0"},null,"RATE ONLY"]
[]
["18.5.2.13",null,"(m) 27t pneumatic roller","h",{"v":0,"d":"0.0"},null,"RATE ONLY"]
[]
["18.5.2.14",null,"(n) Portable diesel compressor 175 cfm with 1 jackhammer and 30m hose","h",{"v":0,"d":"0.0"},null,"RATE ONLY"]
[]
["18.5.2.15",null,"(o) Portable diesel compressor 450 cfm with 3 jackhammers and 90m hose","h",{"v":0,"d":"0.0"},null,"RATE ONLY"]
[]
["18.5.2.16",null,"(p) Flat truck 2-3t","h",{"v":0,"d":"0.0"},null,"RATE ONLY"]
[]
["18.5.2.17",null,"(q)1m wide milling machine","h",{"v":0,"d":"0.0"},null,"RATE ONLY"]
[]
["18.5.2.18",null,"(r) 2m wide milling machine","h",{"v":0,"d":"0.0"},null,"RATE ONLY"]
[]
["18.5.2.19",null,"(s) 4\"water pump","h",{"v":0,"d":"0.0"},null,"RATE ONLY"]
[]
["18.5.2.20",null,"(t) Rotary broom-mechanically operated","h",{"v":0,"d":"0.0"},null,"RATE ONLY"]
[]
["18.5.3","B18.03","Materials"]
[]
["18.5.3.1",null,"(a) Procurement of materials","Prov sum",{"v":1,"d":" 1.0"},{"v":250000,"d":"250,000.00"},{"v":250000,"d":"250,000.00"}]
["18.5.3.2",null,"(b) Contractor's handling costs, profit and all other charges in respect of subitem B1803(a)","%",{"v":250000,"d":"250 000.00"}]
[]
["18.5.4","B18.04","Transport"]
[]
["18.5.4.1",null,"(a) LDV 2000 cc engine capacity","km",{"v":10,"d":" 10.0"}]
[]
["18.5.4.2",null,"(b) Flatbed truck","km",{"v":10,"d":" 10.0"}]
[]
[" Total Carried Forward To Access Road Summary "]
[null,null,"Lethabo Pump Station: ",{"$nulls":3},"Section 19: Access Road"]
[null,null,"Header Upgrade at Lethabo Pumping Station",null,null,"COLTO: ",2100]
[]
["Item No.","Payment Ref."," Description","Unit","Quantity","Rate","Amount R"]
[18.6,2100,"DRAINS"]
[]
["18.6.1","21.01","Excavation for open drains:"]
[]
["18.6.1.1",null,"(a) Excavating soft material situated within the following depth ranges below the surface level:"]
[]
["18.6.1.2",null,"(1) 0 m up to 1,5 m","m³",{"v":50,"d":" 50.0"}]
[]
["18.6.1.3",null,"(b) Extra over subitem B21.01(a) for excavation in hard material, irrespective of depth","m³",{"v":30,"d":" 30.0"}]
[]
["18.6.2",21.02,"Clearing and shaping existing open drains","m³",{"v":10,"d":" 10.0"}]
[]
["18.6.3",21.1,"Synthetic fibre filter fabric (geotextile/ geo synthetic fibre class B)","m²",{"v":150,"d":" 150.0"}]
[]
["18.6.4",21.14,"Repairing or replacing existing drainage systems","Prov sum",{"v":1,"d":" 1.0"},{"v":50000,"d":"50,000.00"},{"v":50000,"d":"50,000.00"}]
[]
["18.6.5",21.16,"Backfilling existing eroded side drains","m³",{"v":25,"d":" 25.0"}]
{"$rows_empty":44}
[" Total Carried Forward To Access Road Summary "]
[]
[null,null,"Lethabo Pump Station: ",{"$nulls":3},"Section 19: Access Road"]
[null,null,"Header Upgrade at Lethabo Pumping Station",null,null,"COLTO: ",2200]
[]
["Item No.","Payment Ref."," Description","Unit","Quantity","Rate","Amount R"]
[18.7,2200,"PREFABRICATED CULVERTS"]
[]
["18.7.1",22.01,"Excavation"]
[]
["18.7.1.1",null,"(a) Excavating soft material situated within the following depth ranges below the surface level:"]
[]
["18.7.1.1.2",null,"(i) 0 m up to 1.5 m","m³",{"v":0,"d":" 0.0"},null,"Rate Only"]
[]
["18.7.1.1.3",null,"(ii) Exceeding 1,5 m and up to 3,0 m","m³",{"v":0,"d":" 0.0"},null,"Rate Only"]
[]
["18.7.1.1.4",null,"(c) Extra over subitem 22.01(a) for excavation in hard material, irrespective of depth","m³",{"v":0,"d":" 0.0"},null,"Rate Only"]
[]
["18.7.2",22.02,"Backfilling:"]
[]
["18.7.2.1",null,"(a) Using the excavated material","m³",{"v":0,"d":" 0.0"},null,"Rate Only"]
[]
["18.7.2.2",null,"(b) Using imported selected material","m³",{"v":0,"d":" 0.0"},null,"Rate Only"]
[]
["18.7.3",22.03,"Concrete pipe culverts:"]
[]
["18.7.3.1",null,"(c) on class C bedding"]
[]
["18.7.3.1.2",null,"(ii) 600mm dia. Spigot and Socket","m",{"v":0,"d":" 0.0"},null,"Rate Only"]
[]
["18.7.3.1.3",null,"(iii) 900mm dia Spigot and Socket","m",{"v":0,"d":" 0.0"},null,"Rate Only"]
[]
[]
[]
["18.7.4",22.05,"Portal and rectangular culverts"]
[]
[null,null,"(b) Without prefabricated floor slabs(600 x 450mm rectangular portal culvert)","m",{"v":0,"d":" 0.0"},null,"Rate Only"]
[]
["18.7.5",22.07,"Cast in situ concrete and formwork"]
[]
["18.7.5.1",null,"(b) In floor slabs for portal or rectangular culverts, including formwork and class U2 surface finish"]
[]
["18.7.5.1.1",null,"(i) Class 25/19","m³",{"v":0,"d":" 0.0"}]
[]
["18.7.6",22.08,"Concrete backfill for pavements (class 25/19)","m³",{"v":0,"d":" 0.0"},null,"Rate Only"]
[]
["18.7.7",22.1,"Steel reinforcement"]
[]
["18.7.7.1",null,"(b) High-tensile steel bars","t",{"v":0,"d":" 0.00"},null,"Rate Only"]
[]
["18.7.8","B22.17","Manholes,chutes,  catchpits, precast inlet and outlet structures complete:"]
[]
["18.7.8.1",null,"(c) Inlet and Outlet structures (headwall and wing wall as per standard detail drawing RA9160/900)","No",{"v":4,"d":" 4.0"}]
[]
["18.7.9","22.26","Hand excavation to determine the position of existing services","m³",{"v":20,"d":" 20.0"}]
{"$rows_empty":9}
[" Total Carried Forward To Access Road Summary "]
[]
[null,null,"Lethabo Pump Station: ",{"$nulls":3},"Section 19: Access Road"]
[null,null,"Header Upgrade at Lethabo Pumping Station",null,null,"COLTO: ",2300]
[]
["Item No.","Payment Ref."," Description","Unit","Quantity","Rate","Amount R"]
[18.8,"B2300","CONCRETE KERBING, CONCRETE CHANNELLING, CHUTES AND DOWNPIPES, AND CONCRETE LININGS FOR OPEN DRAINS"]
[]
["18.8.1",23.01,"Concrete kerbing:"]
[]
["18.8.1.1",null,"(a) Fig 8c kerb as per drawing Nos RA9160/700 & RA9160/900:"]
[]
["18.8.1.1.1",null,"(ii) For radius exceeding 5,0m up to 20,0m ","m",{"v":149,"d":" 149.0"}]
[]
["18.8.1.1.2",null,"(iii) For radius exceeding 20m (straight)","m",{"v":655,"d":" 655.0"}]
[]
["18.8.2","B23.03","Concrete chutes (as per drawing No RA9160/900)"]
[]
["18.8.2.1",null,"(a) In soft material","m",{"v":12,"d":" 12.0"}]
[]
["18.8.3","B23.07","Trimming of excavations for concrete lined open drains\r\n"]
[]
["18.8.3.1",null,"(a) In soft material","m²",90]
[]
["18.8.3.2",null,"(b) Hard material","m²",10]
[]
["18.8.4",23.08,"Concrete lining for open drains"]
[]
["18.8.4.1",null,"(a) Cast in situ concrete lining class 20/19"]
[]
["18.8.4.1.1",null,"(ii) for V-drain as per standard drawings","m³",{"v":12,"d":" 12.0"}]
[]
["18.8.4.2",null,"(b) Class U2 surface finish to cast in situ concrete"]
[]
["18.8.4.2.1",null,"(ii) For V-drain as per standard drawings","m²",{"v":0,"d":" 0.0"},null,"Rate Only"]
["."]
["18.8.5",23.09,"Formwork to cast in situ concrete lining for open drains (Class F2 surface finish)"]
[]
["18.8.5.1",null,"(a) To sides with formwork on the internal face only","m²",{"v":0,"d":" 0.0"},null,"Rate Only"]
[]
["18.8.5.2",null,"(c) To ends of slabs","m²",{"v":0,"d":" 0.0"},null,"Rate Only"]
[]
["18.8.6",23.13,"Polyethylene sheeting (0,15 mm thick) for concrete-lined open drains","m²",{"v":0,"d":" 0.0"},null,"Rate Only"]
[]
["18.8.7","23.16","Demolition and removal of existing channel","m³",{"v":20,"d":" 20.0"}]
[]
["18.8.8","23.17","Demolition and removal of existing kerbs","m",300]
{"$rows_empty":11}
[" Total Carried Forward To Access Road Summary "]
[]
[null,null,"Lethabo Pump Station: ",{"$nulls":3},"Section 19: Access Road"]
[null,null,"Header Upgrade at Lethabo Pumping Station",null,null,"COLTO: ",3200]
[]
["Item No.","Payment Ref."," Description","Unit","Quantity","Rate","Amount R"]
[18.9,3200,"SELECTION, STOCKPILING AND BREAKING-DOWN THE MATERIAL FROM BORROW PITS, CUTTINGS AND EXISTING PAVEMENT LAYERS, AND PLACING AND COMPACTING THE GRAVEL LAYERS"]
[]
["18.9.1",32.04,"Removal of oversize pavement material","m³",{"v":30,"d":" 30.0"}]
[]
["18.9.2",32.06,"Stockpiling of material","m³",{"v":150,"d":" 150.0"}]
{"$rows_empty":58}
[" Total Carried Forward To Access Road Summary "]
[]
[null,null,"Lethabo Pump Station: ",{"$nulls":3},"Section 19: Access Road"]
[null,null,"Header Upgrade at Lethabo Pumping Station",null,null,"COLTO: ",3300]
[]
["Item No.","Payment Ref."," Description","Unit","Quantity","Rate","Amount R"]
[{"v":18.1,"d":"18.10"},3300,"MASS EARTHWORKS"]
[]
["18.10.1","B33.01","Cut and borrow to fill, including free haul"]
[]
["18.10.1.1",null,"(a) Materials in compact layer thickness of 200 mm and less:"]
[]
[null,null,"(i) Compacted to 90% of modified AASHTO density","m³",{"v":413,"d":" 413.0"}]
["18.10.1.1.1"]
["18.10.1.1.2",null,"(iii) Eight roller passes compaction","m³",{"v":11.5,"d":" 11.5"}]
[]
["18.10.2",33.03,"Extra over item 33.01 for excavating and breaking down material in:"]
[]
["18.10.2.1",null,"(a) Intermediate excavation","m³",{"v":100,"d":" 100.0"}]
[]
["18.10.2.2",null,"(b) Hard excavation","m³",{"v":100,"d":" 100.0"}]
[]
["18.10.2.3",null,"(c) Dealing Unforeseen or Abnormal underground water conditions","Prov. Sum",{"v":1,"d":" 1.0"},{"v":250000,"d":"250,000.00"},{"v":250000,"d":"250,000.00"}]
[]
["18.10.3","B33.04","Cut to spoil, including free-haul up to 1,0 km. Material obtained from:"]
[]
["18.10.3.1",null,"(a) Soft excavation","m³",{"v":35,"d":" 35.0"}]
[]
["18.10.3.2",null,"(b) Intermediate excavation","m³",{"v":53,"d":" 53.0"}]
[]
["18.10.3.3",null,"(c) Hard excavation","m³",{"v":88,"d":" 88.0"}]
[]
["18.10.4","B33.07","Removal of unsuitable material (including free-haul of 1,0 km):"]
[]
["18.10.4.1",null,"(a) In layer thicknesses of 200 mm and less:"]
[]
["18.10.4.1.1",null,"(i) Stable material","m³",{"v":50,"d":" 50.0"}]
[]
["18.10.5",33.08,"Widening of cuts (extra over items 33.01, 33.02 and 33.04)"]
[]
["18.10.5.1",null,"(c) In all other materials","m³",{"v":25,"d":" 25.0"}]
[]
["18.10.6",33.09,"Material bladed to windrow","m³",{"v":100,"d":" 100.0"}]
[]
["18.10.7",33.1,"Roadbed preparation and the compaction of material"]
[]
["18.10.7.1",null,"(a) Compaction to 93% of modified AASHTO density","m³",{"v":413,"d":" 413.0"}]
[]
["18.10.8",33.12,"Insitu treatment of Roadbed"]
[]
["18.10.8.1",null,"(a) Insitu treatment by ripping","m²",{"v":2753,"d":"2 753.0"}]
[]
["18.10.9",33.13,"Finishing-off cut and fill slopes, medians and interchange areas:"]
[]
["18.10.9.1",null,"(a) Cut slopes","m²",{"v":429,"d":" 429.0"}]
[]
["18.10.9.2",null,"(b) Fill slopes","m²",{"v":55,"d":" 55.0"}]
[]
["18.10.10",33.14,"Extra-over item 33.01 for excavating material from pavements and fills for existing roads"]
[]
["18.10.10.1",null,"(a) Non-cemented material","m³",{"v":413,"d":" 413.0"}]
[]
["18.10.11",33.16,"Widening of fills as specified in subclause 3307(i) extra over:"]
[]
["18.10.11.1",null,"(a) Item 33.01(a)","m³",{"v":50,"d":" 50.0"}]
[]
["18.10.12","B33.21","Extra over items 33.04 and 33.07 for spoiling materials off site","m³",{"v":200,"d":" 200.0"}]
[]
[" Total Carried Forward To Access Road Summary "]
[]
[null,null,"Lethabo Pump Station: ",{"$nulls":3},"Section 19: Access Road"]
[null,null,"Header Upgrade at Lethabo Pumping Station",null,null,"COLTO: ",3400]
[]
["Item No.","Payment Ref."," Description","Unit","Quantity","Rate","Amount R"]
[18.11,3400,"PAVEMENT LAYERS OF GRAVEL MATERIAL"]
[]
["18.11.1",34.01,"Pavement layers constructed from gravel taken from cut or borrow, including free haul up to 1,0km:"]
[]
["18.11.1.1",null,"(a) G6 Gravel selected layer compacted to:"]
[]
["18.11.1.1.1",null,"(i) 93% of modified AASHTO density (150mm thick)","m³",{"v":374,"d":" 374.0"}]
[]
["18.11.1.1.2",null,"(iii) 95% of modified AASHTO density (150mm thick)","m³",{"v":50,"d":" 50.0"}]
[]
["18.11.1.2",null,"(d) Gravel subbase (chemically stabilised material) compacted to:"]
[]
["18.11.1.2.1",null,"(i) 95% of modified AASHTO density (150mm thick)","m³",{"v":374,"d":" 374.0"}]
[]
["18.11.1.3",null,"(f) Gravel base (chemically stabilised material) compacted to:"]
[]
["18.11.1.3.1",null,"(i) 97% of modified AASHTO density (150mm thick)","m³",{"v":345,"d":" 345.0"},null,"Rate Only"]
[]
["18.11.1.4",null,"(g) Gravel shoulders compacted to:"]
[]
["18.11.1.4.1",null,"(ii) 95% of modified AASHTO density","m³",{"v":149,"d":" 149.0"}]
[]
["18.11.2",34.07,"Extra over item 34.04 for temporarily blading the material to windrow","m³",30]
[]
["18.11.2.1",{"v":34.1,"d":"34.10"},"Compacting the floors of pavement excavations (5 roller passes) with:"]
[]
["18.11.2.1.1",null,"(a) Vibratory rollers","m²",{"v":1100,"d":"1 100.0"}]
[]
["18.11.2.1.2",null,"(b) Oscillatory rollers","m²",550]
[]
["18.11.2.1.3",null,"(e) Pneumatic rollers","m²",{"v":550,"d":" 550.0"}]
[]
["18.11.3",34.11,"Watering the pavement excavation floor","kℓ",{"v":60,"d":" 60.0"}]
[]
["18.11.4",34.12,"Variations in the number of roller passes applicable to item 34.10:"]
[]
["18.11.4.1",null,"(a) Vibratory rollers","m²-pass",{"v":12,"d":" 12.0"}]
[]
["18.11.4.2",null,"(b) Oscillatory rollers","m²-pass",{"v":12,"d":" 12.0"}]
[]
["18.11.4.3",null,"(e) Pneumatic-tyred rollers","m²-pass",{"v":12,"d":" 12.0"}]
[]
["18.11.5","34.14","Extra over item 34.01 for supply of material from commercial sources"]
[]
["18.11.5.1",null,"(a) G5 quality material","m³",{"v":345,"d":" 345.0"}]
[]
["18.11.5.2",null,"(b) G6 quality material","m³",{"v":523,"d":" 523.0"}]
{"$rows_empty":9}
[" Total Carried Forward To Access Road Summary "]
[]
[null,null,"Lethabo Pump Station: ",{"$nulls":3},"Section 19: Access Road"]
[null,null,"Header Upgrade at Lethabo Pumping Station",null,null,"COLTO: ",3500]
[]
["Item No.","Payment Ref."," Description","Unit","Quantity","Rate","Amount R"]
[18.12,"3500","STABILISATION"]
[]
["18.12.1","B35.01","Chemical Stabilisation:"]
[]
["18.12.1.1",null,"(c) Gravel subbase and base, 150mm thick","m³",{"v":719,"d":" 719.0"}]
[]
["18.12.2","B35.02","Chemical Stabilizing agent:"]
[]
["18.12.2.1",null,"(a) CEMII 32.5 A-L cement","ton",{"v":50,"d":" 50.0"}]
[]
["18.12.3","35.04","Provision and application of water for curing","Kilolitre",{"v":29,"d":" 29.0"}]
{"$rows_empty":55}
[" Total Carried Forward To Access Road Summary "]
[]
[null,null,"Lethabo Pump Station: ",{"$nulls":3},"Section 19: Access Road"]
[null,null,"Header Upgrade at Lethabo Pumping Station",null,null,"COLTO: ",5100]
[]
["Item No.","Payment Ref."," Description","Unit","Quantity","Rate","Amount R"]
[18.13,5100,"PITCHING, STONEWORK AND PROTECTION AGAINST EROSION"]
[]
["18.13.1","51.05","Stone pitching"]
[]
["18.13.1.1",null,"(a) Plain pitching:"]
[]
["18.13.1.1.1",null,"(i) Method 1"]
[]
["18.13.1.2",null,"(b) grouted stone pitching","m2",{"v":50,"d":" 50.0"}]
[]
["18.13.2","B51.05","Concrete edge beams"]
[]
["18.13.2.1",null,"(a) Class 30/19 (RA9160/600 drawing)","m³",{"v":5,"d":" 5.0"}]
{"$rows_empty":52}
[" Total Carried Forward To Access Road Summary "]
[]
[null,null,"Lethabo Pump Station: ",{"$nulls":3},"Section 19: Access Road"]
[null,null,"Header Upgrade at Lethabo Pumping Station",null,null,"COLTO: ",5500]
[]
["Item No.","Payment Ref."," Description","Unit","Quantity","Rate","Amount R"]
[18.14,"5400","GUARDRAILS"]
[]
["18.14.1","54.01","Guardrails on timber posts"]
[]
["18.14.1.1",null,"(a) Galvanised","m",150]
[]
["18.14.2",54.03,"Extra over item 54.01 for horizontally","m",{"v":75,"d":" 75.0"}]
[]
["18.14.3",54.04,"End treatments:"]
[]
["18.14.3.1",null,"(a) End wings","No.",{"v":2,"d":" 2.0"}]
[]
["18.14.3.2",null,"(b) Bull noses","No.",{"v":2,"d":" 2.0"}]
[]
["18.14.3.3",null,"(d) End treatments in accordance with the drawings where single guardrail sections are used.","No.",{"v":2,"d":" 2.0"}]
[]
["18.14.4",54.06,"Reflective plates","No.",{"v":40,"d":" 40.0"}]
[]
["18.14.5",54.13,"Steel base plates for timber guardrails","No.",{"v":40,"d":" 40.0"}]
{"$rows_empty":43}
[" Total Carried Forward To Access Road Summary "]
[]
[null,null,"Lethabo Pump Station: ",{"$nulls":3},"Section 19: Access Road"]
[null,null,"Header Upgrade at Lethabo Pumping Station",null,null,"COLTO: ",5600]
[]
["Item No.","Payment Ref."," Description","Unit","Quantity","Rate","Amount R"]
[18.15,5600,"ROAD SIGNS"]
[]
["18.15.1",56.01,"Road sign boards with painted or coloured semi-matt background,Synbols,lettering and borders in semi-matt black or in Class 1 retro-reflective material , where the sign board is constructed from:"]
[]
["18.15.1.1",null,"(c) Prepainted galvanised steel plate (chromadek or approved equivalent):"]
[]
["18.15.1.1.1",null,"(i) Area not exceeding 2m²","m²",{"v":1,"d":" 1.0"}]
[]
["18.15.1.1.2",null,"(ii) Area exceeding 2m² but not 10m²","m²",{"v":15,"d":" 15.0"}]
[]
["18.15.1.2",null,"(d) Prepainted galvanized steel profiles (200mm high chromadek or approved equivalent):"]
[]
["18.15.1.2.1",null,"(i) Area not exceeding 10m²","m²",{"v":10,"d":" 10.0"}]
[]
["18.15.2",56.02,"Extra over item 56.01 for using:"]
[]
["18.15.2.1",null,"(a) Background of retro-reflective material of:"]
[]
["18.15.2.1.1",null,"(ii) Class I","m²",{"v":15,"d":" 15.0"}]
[]
["18.15.2.2",null,"(b) Lettering,symbols,number,arrows,emblems and borders of retro-reflective material:"]
[]
["18.15.1.2.1",null,"(i) Class II","m²",{"v":15,"d":" 15.0"}]
[]
["18.15.3",56.03,"Road sign supports (overhead road sign structures excluded):"]
[]
["18.15.3.1",null,"(b) Timber"]
[]
["18.15.3.1.1",null,"(i) 120 mm dia","m",{"v":25,"d":" 25.0"}]
[]
["18.15.3.1.2",null,"(ii) 160mm dia","m",{"v":25,"d":" 25.0"}]
[]
["18.15.4",56.05,"Excavation and backfilling for road sign supports (not applicable to kilometre posts)","m³",{"v":15,"d":" 15.0"}]
[]
["18.15.5",56.08,"Dismantling,storing and re-erecting road signs with a surface area of:"]
[]
["18.15.5.1",null,"(a) Up to 2m²","No",{"v":3,"d":" 3.0"}]
[]
["18.15.5.2",null,"(b) Exceeding 2m² but not 10m²","No",{"v":1,"d":" 1.0"}]
[]
["18.15.6",56.1,"Danger plates at culverts/structures"]
[]
["18.15.6.1",null,"(a) Up to 2m²","No",{"v":20,"d":" 20.0"}]
[]
["18.15.6.2",null,"(b) Exceeding 2m² but not 10m²","No",{"v":5,"d":" 5.0"}]
{"$rows_empty":12}
[" Total Carried Forward To Access Road Summary "]
[]
[null,null,"Lethabo Pump Station: ",{"$nulls":3},"Section 19: Access Road"]
[null,null,"Header Upgrade at Lethabo Pumping Station",null,null,"COLTO: ",5700]
[]
["Item No.","Payment Ref."," Description","Unit","Quantity","Rate","Amount R"]
[18.16,5700,"ROAD MARKINGS"]
[]
["18.16.1",57.02,"Retro-reflective road marking paint:"]
[]
["18.16.1.1",null,"(a) White lines (broken or unbroken)"]
[]
["18.16.1.1.1",null,"(i) 150 mm wide","km",{"v":0.5,"d":" 0.5"}]
[]
["18.16.1.1.2",null,"(ii) 200 mm wide","km",{"v":0.2,"d":" 0.2"}]
[]
["18.16.1.1.3",null,"(iii) 500 mm wide","km",{"v":0.1,"d":" 0.1"}]
[]
["18.16.1.2",null,"(d) White lettering and symbols","m²",{"v":30,"d":" 30.0"}]
[]
["18.16.1.3",null,"(e) Yellow lettering and symbols","m²",{"v":5,"d":" 5.0"}]
[]
["18.16.2",57.04,"Variations in rate of application:"]
[]
["18.16.2.1",null,"(a) White paint","litre",{"v":10,"d":" 10.0"}]
[]
["18.16.2.2",null,"(b) Yellow paint","litre",{"v":5,"d":" 5.0"}]
[]
["18.16.2.3",null,"(d) Retro-reflective beads","kg",{"v":10,"d":" 10.0"}]
[]
["18.16.3",57.06,"Setting out and premarking the lines (Excluding traffic-island markings, lettering and symbols)","km",0.5]
[]
["18.16.4",57.07,"Re-establishing the painting unit at the end of the maintenance period"]
[]
["18.16.4.1",null,"(a) Overpainting as temporary measure","L/sum",{"v":1,"d":" 1.0"},{"v":50000,"d":"50 000.00"},{"v":50000,"d":"50 000.00"}]
{"$rows_empty":35}
[" Total Carried Forward To Access Road Summary "]
[]
[null,null,"Lethabo Pump Station: ",{"$nulls":3},"Section 19: Access Road"]
[null,null,"Header Upgrade at Lethabo Pumping Station",null,null,"COLTO: ",5900]
[]
["Item No.","Payment Ref."," Description","Unit","Quantity","Rate","Amount R"]
[18.17,5900," FINISHED THE ROAD AND ROAD RESERVE AND TREATING OLD ROADS"]
[]
["18.17.1",59.01,"Finishing the road and road reserve:"]
[]
["18.17.1.1",null,"(b) Single carriageway road","km",{"v":0.6,"d":" 0.6"}]
[]
["18.17.2",59.02,"Treatment of old roads and temporary deviations","km",{"v":0.6,"d":" 0.6"}]
{"$rows_empty":58}
[" Total Carried Forward To Access Road Summary "]
[]
[]
[null,null,"Lethabo Pump Station: ",{"$nulls":3},"Section 19: Access Road"]
[null,null,"Header Upgrade at Lethabo Pumping Station",null,null,"COLTO: ",7300]
[]
["Item No.","Payment Ref."," Description","Unit","Quantity","Rate","Amount R"]
[18.18,"7300","CONCRETE BLOCK PAVING FOR ROADS"]
[]
["18.18.1","73.01","Concrete interlocking block paving, 80mm thick","m²",{"v":2500,"d":"2 500.0"}]
[]
["18.18.2","73.02","Cast in situ concrete edge and intermediate beams","m³",{"v":5,"d":" 5.0"}]
[]
["18.18.3","73.03","Provision of approved herbicide and ant poison:"]
[]
["18.18.3.1",null,"(a) Provision of materials","PC Sum ",1,null,{"v":75000,"d":"75 000.00"}]
[]
["18.18.3.2",null,"(b) Profit","%",{"v":75000,"d":"75 000.00"}]
{"$rows_empty":54}
[" Total Carried Forward To Access Road Summary "]
[]
[null,null,"Lethabo Pump Station: ",{"$nulls":3},"Section 19: Access Road"]
[null,null,"Header Upgrade at Lethabo Pumping Station",null,null,"COLTO: ",8100]
[]
["Item No.","Payment Ref."," Description","Unit","Quantity","Rate","Amount R"]
[18.19,"8100","TESTING MATERIALS AND WORKMANSHIP"]
[]
["18.19.1","81.02","Other special tests requested by the engineer"]
[]
["18.19.1.1",null,"(a) Cost of testing","PC Sum",{"v":1,"d":" 1.0"},null,{"v":100000,"d":"100 000.00"}]
[]
["18.19.2","81.03","Providing testing equipment"]
[]
["18.19.2.1",null,"(a) Rolling straight-edge","No",2]
{"$rows_empty":56}
[" Total Carried Forward To Access Road Summary "]
[]
[]
[null,null,"Lethabo Pump Station: "]
[null,null,"Header Upgrade at Lethabo Pumping Station"]
[]
["ACCESS ROAD SUMMARY "]
[null,"Section","Description"," "," "," ","Amount R"]
[]
[null,"1200","GENERAL REQUIREMENTS AND PROVISIONS"]
[]
[null,1300,"GENERAL REQUIREMENTS"]
[]
[null,1500,"ACCOMODATION OF TRAFFIC"]
[]
[null,1700,"CLEARING AND GRUBBING"]
[]
[null,1800," DAYWORK"]
[]
[null,2100,"DRAINS"]
[]
[null,2200,"PREFABRICATED CULVERTS"]
[]
[null,"B2300","CONCRETE KERBING, CONCRETE CHANNELLING, CHUTES AND DOWNPIPES, AND CONCRETE LININGS FOR OPEN DRAINS"]
[]
[null,3200,"SELECTION, STOCKPILING AND BREAKING-DOWN THE MATERIAL FROM BORROW PITS, CUTTINGS AND EXISTING PAVEMENT LAYERS, AND PLACING AND COMPACTING THE GRAVEL LAYERS"]
[]
[null,3300,"MASS EARTHWORKS"]
[]
[null,3400,"PAVEMENT LAYERS OF GRAVEL MATERIAL"]
[]
[null,"3500","STABILISATION"]
[]
[null,5100,"PITCHING, STONEWORK AND PROTECTION AGAINST EROSION"]
[]
[null,"5400","GUARDRAILS"]
[]
[null,5600,"ROAD SIGNS"]
[]
[null,5700,"ROAD MARKINGS"]
[]
[null,5900,"FINISHED THE ROAD AND ROAD RESERVE AND TREATING OLD ROADS"]
[]
[null,7300,"CONCRETE BLOCK PAVING FOR ROADS"]
[]
[null,8100,"TESTING MATERIALS AND WORKMANSHIP"]
[]
[null,"Section 18 Subtotal Carried Forward to Summary"]

{"sheet":"20. SED","index":20,"n_rows":42,"n_cols":9,"rows_kept":42,"merged":[[41,0,41,4]],"flags":["formulas_cached_only"]}
[]
[]
[]
["SECTION 20: SKILLS DEVELOPMENT PROGRAM"]
["ITEM NO.","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null," "]
[20.1,"SKILLS DEVELOPMENT PROGRAM"]
[]
[{"$nulls":8},1.5]
[]
[]
[]
[20.2,"SOCIAL RESPONSIBILITY PROGRAM"]
[]
[]
[]
["20.2.2","Contractors mark-up on Item 20.2.1 above","%"]
[]
[20.3,"COMMUNITY LIASON OFFICER"]
[]
["20.3.1","Community Liason Officer. A key component in aiding the realisation of the SED objectives is effective community liaison with all the relevant role-players, structures, civic organisations and the community at large. \n(The Bidder to input a sum that comprises the salary that would be paid to the CLO)","PSum",1,{"v":0.005,"d":"0.50%"}]
[]
["20.3.2","Contractors mark-up on Item 20.3.1 above","%"]
[]
[20.4,"SED ADMINISTRATION"]
[]
["20.4.1","Labour Management Services (1% of Project Value - Sub Total A)","PSum",null,{"v":0.01,"d":"1%"}]
[]
["20.4.2","Contractors mark-up on Item 20.4.1 above","%"]
[]
[20.5,"PARTICIPATION OF LOCAL ENTERPRICES"]
[]
["20.5.1","Work Allocated to Local Enterprises  (Inclusive of P&G's and SHEQ) (Minimum 5% of Project Value) (Sub-Total A)","PSum",1,null,"Rate Only"]
[]
["20.5.2","Contractors mark-up on Item 20.5.1 above","%"]
[]
[]
[]
[]
[]
[]
["SECTION 18:  TOTAL CARRIED FORWARD TO SUMMARY "]

{"sheet":"21.Summary","index":21,"n_rows":75,"n_cols":3,"rows_kept":75,"merged":[[33,5,33,7],[48,0,48,1],[51,0,51,1],[52,0,52,1],[53,0,53,1],[56,0,56,1],[59,0,59,1],[62,0,62,1],[65,0,65,1],[66,0,66,1],[67,0,67,1],[70,0,70,1],[72,0,72,2],[74,0,74,2]],"flags":["formulas_cached_only"]}
[null,"Lethabo Pump Station "]
[null,"ethabo Pumping Station Upgrade "]
[]
["Section","Description                                 SUMMARY  ","AMOUNT"]
[]
[1,"PRELIMINARY AND GENERAL","R                       -"]
[]
[2,"PROVISIONAL SUMS","R                       -"]
[]
[3,"SAFETY AND HEALTH","R                       -"]
[]
[4,"ENVIRONMENTAL","R                       -"]
[]
["4B","QUALTY CONTROL AND ASSURANCE ","R                       -"]
[]
[5,"DAYWORKS","R                       -"]
[]
[6,"CIVIL - SITE CLEARANCE","R                       -"]
[]
[7,"CIVIL - EARTHWORKS","R                       -"]
[]
[8,"CIVIL - CONCRETE","R                       -"]
[]
[9,"CIVIL - PRECAST CONCRETE","R                       -"]
[]
[10,"CIVIL - STRUCTURAL STEEL","R                       -"]
[]
[11,"PIPELINE - SITE CLEARANCE","R                       -"]
[]
[12,"PIPELINE - EARTHWORKS & BEDDING","R                       -"]
[]
[13,"PIPELINE - PIPES AND SPECIALS","R                       -"]
[]
[14,"PIPELINE - PIPE SPECIALS M & V","R                       -"]
[]
[15,"PIPELINE - PIPELINE SUNDRIES","R                       -"]
[]
[16,"CATHODIC PROTECTION","R                       -"]
[]
[17,"MECHANICAL HEADER","R                       -"]
[]
[18,"PUMPS & ROTARY SCREENS ","R                       -"]
[]
[19,"ACCESS ROAD","R                       -"]
[]
[20,"SED ","R                       -"]
[]
[]
["SUBTOTAL A ……………………………………..……………………………………………",null,"R                       -"]
[]
[]
["CONTINGENCIES"]
["Add 10% of SUBTOTAL A …………..…………………...…...…………………………….",null,"R                       -"]
["(The Provisional Sum provided here may only be expended at the sole discretion of the Engineer, and the Employer reserves the right, during the execution of the works, to adjust the stated sum downwards or to omit it entirely without affecting the validity of the contract.)"]
[]
[]
["SUBTOTAL B ……..…………..………………………..………….…………………………",null,"R                       -"]
[]
[]
["CONTRACT PRICE ADJUSTMENT (Provisional Allowance)………………………….."]
[]
[]
["SUBTOTAL C ……………………...…..……………………………….……………………."]
[]
[]
["VALUE ADDED TAX"]
["Add 15% of Subtotal C ………..…….……………………..………...……..………………"]
["(Provisional sum based on current rate of VAT)"]
[]
[]
["TOTAL CARRIED TO FORM C1.1, FORM OF OFFER"]
[]
[]
[]
["SIGNED ON BEHALF OF TENDERER: ……………………………………………..……………………………………………."]

{"sheet":"Sheet1","index":22,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}