{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["KPA"],"not_rendered":{"external_links":3,"defined_names":17},"read":"whole","date_system":"1900"}

{"sheet":"KPA","index":0,"n_rows":137,"n_cols":7,"rows_kept":137}
["ITEM NO","LOCATION","DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT"]
[]
[null,null,"Building External Finishes "]
[]
[null,null,"Location Key"]
[null,"L1","All Areas"]
[null,null,"The Model Preambles for Trades as published by the Association of South African Quanity Surveyors shall be deemed to be incorporated in these bills of and no claims arising from brevity of description of items fully described in the said Model Preamble will be entertained."]
[]
[null,null,"The contractors prices for all items throughout these bills of quanities shall take account of and include for all of the obligations, requirements and specifications given in the Model Preambles and in any supplementary preamble"]
[]
[1,null,"Preliminaries and General"]
[]
[null,"L1","Insurance - Value Related","Month",{"v":1,"d":"1.00"},"R","R"]
[null,"L1","OHS Related Safety Charges - Value Related","Month",{"v":1,"d":"1.00"},"R","R"]
[null,"L1","Contractors site establishment - Fixed Costs ","Month",{"v":1,"d":"1.00"},"R","R"]
[null,"L1","Contractors contractual obligations including cleaning de-establishing site upon completion - Value Related","Month",{"v":1,"d":"1.00"},"R","R"]
[null,"L1","ACSA Issue Permits & Induction Costs - Reimbursed Based on Proven Costs - No Mark Up Allowed","Prov Sum",{"v":1,"d":"1.00"},{"v":30000,"d":"R30,000.00"},{"$f":"E17*F17","v":{"v":30000,"d":"R30,000.00"}}]
[]
[2,null,"ALTERATIONS"]
[]
[null,null,"SUPPLEMENTARY PREAMBLES"]
[]
[null,null,"Tenderers are refered to \"Department of Public Works:\nSpecification of materials and methods to be used -\nPW371-A\" for preambles."]
[]
[null,null,"General"]
[]
[null,null,"The Supplementary Preambless reflected elsewhere in these Bills of Quantities shall apply equally to this Trade."]
[null,null,"Contractors to factor in necessary scaffolding etc for working at heights in rates, no additional costs will be entertained."]
[]
[null,null,"Damage and repairs to services:"]
[]
[null,null,"Should the contractor damage any services which are to remain in operation or any services which have not yet been disconnected prior to removal, then the Contractor will be held solely responsible for such damage and any further resultant damage."]
[]
[null,null,"The Contractor shall immediately notify the Representative/Agent and the Authorities concerned\nand shall at his own cost make all necessary arrangements for disconnection and repairs with the\nrelevant authorities and shall pay all fees and charges levied."]
[null,null,"Demolitions and work on site:"]
[]
[null,null,"All demolitions and work on site must be carried out carefully and in the safest possible manner and the Contractor is to make a thorough examination and take all necessary precautions before proceeding with the work. The outmost care is to be observed to avoid any structural or other damage in the remaining portions of the existing buildings."]
[]
[null,null,"Special care must be exercised as not to interfere with any electrical installation, and notice is to given to the Representative/Agent when any disconnections, removal of wire, etc, are necessary and the Contractor is to afford every facility to the workmen carrying out the work."]
[]
[null,null,"Disposal of material"]
[]
[null,null,"All existing materials specified as 'removed' \"demolished and removed\", \"hacked up or off and removed\" or \"taken down or off and removed\" or \"broken down and removed\", etc. become the property of the Contractor."]
[]
[null,null,"If any of the bricks or other material specified to be \"removed\" are sound and considered suitable for any portion of the new work they must be thoroughly cleaned off, stackered on site for inspection by the Representative/Agent must be obtained before any such materials are re-used in the work."]
[null,null,"All existing materials specified to be \"taken down and set aside for re-use\" or \"taken down and set aside\" shall remain the property of the Employer and must be cleaned off, cleared of all nails, etc., and neatly stacked and stored on site by the Contractor where directed and carefully handled during taking down, storage and refixing. The Contractor will be held responsible for the safety of these materials and must take all necessary pre-cautions for their protecction and any damage or loss that may occur maust be made good by the Contractor at his own expense."]
[]
[null,null,"REMOVAL OF EXISTING WORK"]
[]
[null,null,"Taking out/off and removing sundry metalwork"]
[]
[null,"L1","Steel Louvrers 850mm high to Aluminium windows, including bracing and all accessories etc complete","m",{"v":284,"d":"284.00"},"R","R"]
[null,null,"Recovering cost of selling/disposing metal offsite","Item",{"v":1,"d":"1.00"},"R","R"]
[]
[null,null,"Carefully taking out/off and removing sundry metalwork and set aside for re-use(elsewhere measured)"]
[]
[null,"L1","Steel Awnings n.e 1200mm high to Aluminium windows, including bracing and all accessories etc complete","m",{"v":110,"d":"110.00"},"R","R"]
[]
[3,null,"METALWORKS"]
[]
[null,null,"Preambles"]
[null,null,"The contractor is refered to the relevant clause in the document Model Preambles for Trades as published by the Association of South African Quanitity Surveyors as amended"]
[]
[null,null,"Supplementary Preambles"]
[null,null,"Descriptions of bolts, anchors, etc"]
[]
[null,null,"Descriptions shall be deemed to include bolts, nuts and washers, anchors, chemical anchors and mortices in brickwork or concrete"]
[]
[null,null,"Louvre Units"]
[null,null,"Modular louvres including frames to specialist detail. The contractor will be required to provide concept designs and shop drawings for client approval."]
[]
[null,null,"Provide the sum of R500 000.00 for louvre units","Prov Sum",{"v":1,"d":"1.00"},"R","R"]
[null,null,"Provide for profit & attendance","Iten",{"v":1,"d":"1.00"},"R","R"]
[]
[]
[4,null,"EXTERNAL WORKS"]
[]
[null,null,"ROADWORK, PARKING AREAS AND PAVING"]
[]
[null,null,"Alterations"]
[]
[null,null,"Break up and remove existing stone paving and prepare to receive new","m2",{"v":1004,"d":"1004.00"},"R","R"]
[]
[null,null,"Earthworks"]
[]
[null,null,"Site Clearance"]
[]
[null,null,"Digging up and removing rubbish, debris, vegetation, hedges, shrubs and trees not exceeding 200mm girth, bush, etc.","m2",{"v":1004,"d":"1004.00"},"R","R"]
[]
[null,null,"Stripping average 500mm thick layer of top soil and stockpiling on site (LI)","m2",{"v":1004,"d":"1004.00"},"R","R"]
[]
[null,null,"Open face excavation not exceeding 2m deep:"]
[]
[null,null,"Over site to reduce levels and depositing excavated material in prescribed stock piles on site.","m3",{"v":301,"d":"301.00"},"R","R"]
[]
[null,null,"Risk of Collapse ","m2",{"v":64,"d":"64.00"},"R","R"]
[]
[null,null,"KEFFW","Item",{"v":1,"d":"1.00"},"R","R"]
[]
[null,null,"Brick-on-edge header course coping, sills, etc of \" corobrick golden wheat Travertine or similar approved \" face bricks pointed with recessed joints on all exposed faces"]
[]
[null,null,"150mm insitu material, supplied and carted onto the site by the Contractor, compacted to 90% modified AASHTO under solid floors. (LI)"]
[]
[null,null,"Under floors, steps, paving, etc","m3",{"v":89,"d":"89.00"},"R","R"]
[]
[]
[null,null,"20mm Coarse river sand filling supplied by the contractor, compacted to 100% Mod AASHTO density"]
[]
[null,null,"Under floors (LI)    ","m2",{"v":1004,"d":"1004.00"},"R","R"]
[]
[null,null,"Compaction Surfaces:"]
[]
[null,null,"Compaction of ground surface under roads etc including scarifying for a depth of 150mm, breaking down oversize material, adding suitable material from excavated material where necessary and compacting to 93% Mod AASHTO density.","m2",{"v":1004,"d":"1004.00"},"R","R"]
[]
[null,null,"300 x 400 x 100 mm  \"Bosun \" Urban Large pavers or similar approved interlocking paving"]
[]
[null,null,"Paving to parking areas etc to falls on 50mm thick clean river sand (preparation of ground or filling elsewhere measured)","m2",{"v":1004,"d":"1004.00"},"R","R"]
[]
[null,null,"BENCHES, TABLES, ETC"]
[]
[null,null,"\"Old World Concretes\" garden furniture with brown\nexposed aggregate finish to precast concrete\ncomponents, including excavation, backfilling and\nunreinforced concrete footing where applicable"]
[]
[null,null,"Benches 435 x 1 800 x 455mm high","No",{"v":5,"d":"5.00"},"R","R"]
[]
[null,null,"Round concrete litter bins, size 495 diameter x 760mm\nhigh","No",{"v":5,"d":"5.00"},"R","R"]
[]
[]
[null,null,"PRICE SUMMARY"]
["A",null,"SUB TOTAL FOR THE WORKS - EXCLUDING VAT",{"$nulls":3},"R"]
[]
["B",null,"CONTINGENCIES - 10%  OF A",{"$nulls":3}," R"]
[]
["C",null,"SUB TOTAL FOR THE WORKS INCLUDING CONTINGENCIES - EXCLUDING VAT - A + B",{"$nulls":3},"R"]
[]
["D",null,"VALUE ADDED TAX - VAT AT 15% OF C",{"$nulls":3},"R"]
[]
["E",null,"TOTAL PRICE FOR THE WORKS - INCLUDING VAT  - C + D ( Price transferred to Form of Offer) ",{"$nulls":3},"R"]