{"text_format":"3","workbook":"xlsx","n_sheets":5,"sheets":["Botshabelo","Mulamula","Oliphantshoek","Tshitale","Vuwani"],"read":"whole","date_system":"1900"}

{"sheet":"Botshabelo","index":0,"n_rows":113,"n_cols":3,"rows_kept":113,"merged":[[27,0,27,2],[43,0,43,2],[57,0,57,2],[71,0,71,2],[85,0,85,2]]}
["Item","Description","QTY"]
[null,"Limpopo LSAC:Provincial Archive Building"]
[null,"1. Sever room"]
[1,"Krone UTP CAT6 Data Point complete with 3m flylead and patchlead",2]
[2,"ADAPTER 22.5 X 45 LEGRAND HK SHUTTER",2]
[{"$f":"A5+1","v":3},"KEYSTONE RJ45 KM8 C6 WHITE STP",2]
[4,"Cover Plate P/O 50x50 E/O",2]
[5,"Collar 50x50",2]
[6,"Euromod Half Blank White",2]
[7,"Electrical Normal Power Point  complete, excl CB.",5]
[8,"Electrical Dedicated Power Point  complete, excl CB.",5]
[9,"Cover 2 X 4 Vert White 16 Amp",5]
[10,"Cover Socket 2 X 4 Vert Red Ded 16 Amp For MS2",5]
[11,"Plugtop 16 Amp Red",5]
[12,"Cable Surfex 6 X 2 Core + Earth","40m"]
[13,"Cable Surfex 2.5 X 2 Core + Earth dedicated plugs & normal plugs","20m"]
[14,"Dual Metal Channel (Incl Corners, End Caps Etc.) Easter Oak / Hospital Grey","9m"]
[15,"Switches 48 PORT",2]
[16,"BRADY \"0\" - \"9\" 37/STRIP BLACK/WHITE",2]
[17,"BRUSH PANEL SHORT BASE METAL",8]
[18,"24 PORT PATCH PANEL CAT 6e LOADED",4]
[19,"43U Cabinet. (Includes UPS, power surge protection, cabinet management, etc.)",1]
[20,"Smart-UPS, 900 Watts /1500 VA, Input 230V /Output 230V, Interface Port USB, Floor Standing",1]
[21,"Distribution Cabinet, Surface Mountable, White, 24 WAY",1]
[22,"60a, Earth Leakage",1]
[23,"60a 1 Phase CB/Isolator",1]
[24,"25a, Circuit Breaker, Std Curve",15]
["2. COMPUTER ROOM"]
[1,"Krone UTP CAT6 Data Point complete with 3m flylead and patchlead",30]
[{"$f":"A29+1","v":2},"ADAPTER 22.5 X 45 LEGRAND HK SHUTTER",30]
[{"$f":"A30+1","v":3},"KEYSTONE RJ45 KM8 C6 WHITE STP",30]
[{"$f":"A31+1","v":4},"Cover Plate P/O 50x50 E/O",30]
[{"$f":"A32+1","v":5},"Collar 50x50",30]
[{"$f":"A33+1","v":6},"Acess point for WIFI AP, Surface mount CAT 6 Wall box",1]
[7,"Euromod Half Blank White",30]
[8,"Electrical Normal Power Point  complete, excl CB.",30]
[9,"Electrical Dedicated Power Point  complete, excl CB.",30]
[10,"Cover 2 X 4 Vert White 16 Amp",30]
[11,"Cover Socket 2 X 4 Vert Red Ded 16 Amp For MS2",30]
[12,"Plugtop 16 Amp Red",30]
[13,"Cable Surfex 2.5 X 2 Core + Earth Dedicated plugs & normal plugs","120m"]
[14,"Dual Metal Channel (Incl Corners, End Caps Etc.) Easter Oak / Hospital Grey","20m"]
[]
["3. STUDY SPACE"]
[1,"Krone UTP CAT6 Data Point complete with 3m flylead and patchlead",32]
[{"$f":"A45+1","v":2},"ADAPTER 22.5 X 45 LEGRAND HK SHUTTER",32]
[{"$f":"A46+1","v":3},"KEYSTONE RJ45 KM8 C6 WHITE STP",32]
[{"$f":"A47+1","v":4},"Cover Plate P/O 50x50 E/O",32]
[{"$f":"A48+1","v":5},"Collar 50x50",32]
[{"$f":"A49+1","v":6},"Euromod Half Blank White",32]
[7,"Electrical Normal Power Point  complete, excl CB.",32]
[8,"Electrical Dedicated Power Point  complete, excl CB.",32]
[9,"Cover 2 X 4 Vert White 16 Amp",32]
[10,"Cover Socket 2 X 4 Vert Red Ded 16 Amp For MS2",32]
[11,"Plugtop 16 Amp Red",32]
[12,"Cable Surfex 2.5 X 2 Core + Earth Dedicated plugs & normal plugs","240m"]
[13,"Dual Metal Channel (Incl Corners, End Caps Etc.) Easter Oak / Hospital Grey","20m"]
["4. CHILDREN'S ROOM"]
[1,"Krone UTP CAT6 Data Point complete with 3m flylead and patchlead",6]
[{"$f":"A59+1","v":2},"ADAPTER 22.5 X 45 LEGRAND HK SHUTTER",6]
[{"$f":"A60+1","v":3},"KEYSTONE RJ45 KM8 C6 WHITE STP",6]
[{"$f":"A61+1","v":4},"Cover Plate P/O 50x50 E/O",6]
[{"$f":"A62+1","v":5},"Collar 50x50",6]
[{"$f":"A63+1","v":6},"Euromod Half Blank White",6]
[7,"Electrical Normal Power Point  complete, excl CB.",6]
[8,"Electrical Dedicated Power Point  complete, excl CB.",6]
[9,"Cover 2 X 4 Vert White 16 Amp",6]
[10,"Cover Socket 2 X 4 Vert Red Ded 16 Amp For MS2",6]
[11,"Plugtop 16 Amp Red",6]
[12,"Cable Surfex 2.5 X 2 Core + Earth Dedicated plugs & normal plugs","120m"]
[13,"Dual Metal Channel (Incl Corners, End Caps Etc.) Easter Oak / Hospital Grey","10M"]
["5. LIBRARIAN OFFICE"]
[1,"Krone UTP CAT6 Data Point complete with 3m flylead and patchlead",6]
[{"$f":"A73+1","v":2},"ADAPTER 22.5 X 45 LEGRAND HK SHUTTER",6]
[{"$f":"A74+1","v":3},"KEYSTONE RJ45 KM8 C6 WHITE STP",6]
[{"$f":"A75+1","v":4},"Cover Plate P/O 50x50 E/O",6]
[{"$f":"A76+1","v":5},"Collar 50x50",6]
[{"$f":"A77+1","v":6},"Euromod Half Blank White",6]
[7,"Electrical Normal Power Point  complete, excl CB.",6]
[8,"Electrical Dedicated Power Point  complete, excl CB.",6]
[9,"Cover 2 X 4 Vert White 16 Amp",6]
[10,"Cover Socket 2 X 4 Vert Red Ded 16 Amp For MS2",6]
[11,"Plugtop 16 Amp Red",6]
[12,"Cable Surfex 2.5 X 2 Core + Earth Dedicated plugs & normal plugs","120m"]
[13,"Dual Metal Channel (Incl Corners, End Caps Etc.) Easter Oak / Hospital Grey","15M"]
["6. RECEPTION"]
[1,"Krone UTP CAT6 Data Point complete with 3m flylead and patchlead",8]
[{"$f":"A87+1","v":2},"ADAPTER 22.5 X 45 LEGRAND HK SHUTTER",8]
[{"$f":"A88+1","v":3},"KEYSTONE RJ45 KM8 C6 WHITE STP",8]
[{"$f":"A89+1","v":4},"Cover Plate P/O 50x50 E/O",8]
[{"$f":"A90+1","v":5},"Collar 50x50",8]
[{"$f":"A91+1","v":6},"Acess point for WIFI AP, Surface mount CAT 6 wall box",1]
[7,"Euromod Half Blank White",8]
[8,"Electrical Normal Power Point  complete, excl CB.",8]
[9,"Electrical Dedicated Power Point  complete, excl CB.",8]
[10,"Cover 2 X 4 Vert White 16 Amp",8]
[11,"Cover Socket 2 X 4 Vert Red Ded 16 Amp For MS2",8]
[12,"Plugtop 16 Amp Red",8]
[13,"Cable Surfex 2.5 X 2 Core + Earth Dedicated plugs & normal plugs","60m"]
[14,"Dual Metal Channel (Incl Corners, End Caps Etc.) Easter Oak / Hospital Grey","15M"]
[null,"SUNDRIES/ Infrasrtucture"]
[{"$f":"A101+1","v":1},"Tape Brother White 9mm / BRADY \"0\" - \"9\" 37/STRIP BLACK/WHITE",2]
[2,"Insulation Tape - Black",2]
[3,"Knock Inns 6 X 55",300]
[4,"M6 Flat Washer",100]
[5,"Silicone",3]
[null,"Documentation"]
[{"$f":"A107+1","v":1},"Test Data Point",86]
[2,"UTP Labelling",172]
[3,"Power Labelling",172]
[4,"Schematic Layout Of Network",3]
[5,"Data Certification",1]
[6,"COC - Electrical Certification",1]

{"sheet":"Mulamula","index":1,"n_rows":121,"n_cols":5,"rows_kept":121}
["Item",null,"Description",null,"QTY"]
[null,null,"Mulamula Library"]
[1,null,"Reception Area"]
["1.1","Point","UTP CAT6e Data Point complete with flylead and patchlead","Per Point",3]
["1.2","Frame module","45deg ADAPTER PLATE for COMPACT","Each",3]
["1.3","module","RJ 45 WHITE SHUTTER CAT 6 ","Each",3]
["1.4","frame","TRUNKING FRAME 50 x 50","Each",3]
["1.5","Blank blate","25 X 50 BLANK ","Each",3]
["1.6","Point","Electrical Dedicated Power Point  complete, excl CB.","Per Point",3]
["1.7","Power","15a Dedicated Plugtop","Each",3]
["1.8","Power","15a Plug Assembly, Dedicated Power, Color Red, For Mounting In P801 Metal Skirting","Each",3]
["1.9","Power","Wire, Electrical, Surfex, 2.5 Mm2(Normal Plugs)","P/M",80]
["1.10","Point","Electrical Normal Power Point  complete, excl CB.","Per Point",3]
["1.11","Power","15a Standard Plugtop","Each",3]
["1.12","Power","15a Plug Assembly, Normal Power,  For Mounting In P801 Metal Skirting","Each",3]
["1.13","Power","Wire, Electrical, Surfex, 2.5 Mm2(Red Plugs)","P/M",80]
["1.14","Infrast","Dual Metal Channel  (Incl Corners, End Caps Etc)","P/M",60]
[2,null,"Librarian Office"]
["2.1","Point","UTP CAT6e Data Point complete with flylead and patchlead","Per Point",3]
["2.2","Frame module","45deg ADAPTER PLATE for COMPACT","Each",3]
["2.3","module","RJ 45 WHITE SHUTTER CAT 6 ","Each",3]
["2.4","frame","TRUNKING FRAME 50 x 50","Each",3]
["2.5","Blank blate","25 X 50 BLANK ","Each",3]
["2.6","Point","Electrical Dedicated Power Point  complete, excl CB.","Per Point",3]
["2.7","Power","15a Dedicated Plugtop","Each",3]
["2.8","Power","15a Plug Assembly, Dedicated Power, Color Red, For Mounting In P801 Metal Skirting","Each",3]
["2.9","Power","Wire, Electrical, Surfex, 2.5 Mm2(Normal Plugs)","P/M",80]
["2.10","Point","Electrical Normal Power Point  complete, excl CB.","Per Point",3]
["2.11","Power","15a Standard Plugtop","Each",3]
["2.12","Power","15a Plug Assembly, Normal Power,  For Mounting In P801 Metal Skirting","Each",3]
["2.13","Power","Wire, Electrical, Surfex, 2.5 Mm2(Red Plugs)","P/M",80]
["2.14","Infrast","Dual Metal Channel  (Incl Corners, End Caps Etc)","P/M",60]
[3,null,"Computer Room"]
["3.1","Point","UTP CAT6e Data Point complete with flylead and patchlead","Per Point",18]
["3.2","Frame module","45deg ADAPTER PLATE for COMPACT","Each",18]
["3.3","module","RJ 45 WHITE SHUTTER CAT 6 ","Each",18]
["3.4","frame","TRUNKING FRAME 50 x 50","Each",18]
["3.5","Blank blate","25 X 50 BLANK ","Each",18]
["3.6","Point","Electrical Dedicated Power Point  complete, excl CB.","Per Point",18]
["3.7","Power","15a Dedicated Plugtop","Each",18]
["3.8","Power","15a Plug Assembly, Dedicated Power, Color Red, For Mounting In P801 Metal Skirting","Each",18]
["3.9","Power","Wire, Electrical, Surfex, 2.5 Mm2(Normal Plugs)","P/M",140]
["3.10","Point","Electrical Normal Power Point  complete, excl CB.","Per Point",18]
["3.11","Point","Electrical 2 Pin 5 A Power outlet.","Per Point",2]
["3.12","Power","15a Standard Plugtop","Each",18]
["3.13","Power","15a Plug Assembly, Normal Power,  For Mounting In P801 Metal Skirting","Each",18]
["3.14","Power","Wire, Electrical, Surfex, 2.5 Mm2(Red Plugs)","P/M",140]
["3.15","Infrast","Dual Metal Channel  (Incl Corners, End Caps Etc)","P/M",160]
["3.16","Point","Wifi/APS Connectors","Per Point",1]
[4,null,"Activity Room"]
["4.1","Point","UTP CAT6e Data Point complete with flylead and patchlead","Per Point",21]
["4.2","Frame module","45deg ADAPTER PLATE for COMPACT","Each",21]
["4.3","module","RJ 45 WHITE SHUTTER CAT 6 ","Each",21]
["4.4","frame","TRUNKING FRAME 50 x 50","Each",21]
["4.5","Blank blate","25 X 50 BLANK ","Each",21]
["4.6","Point","Electrical Dedicated Power Point  complete, excl CB.","Per Point",21]
["4.7","Power","15a Dedicated Plugtop","Each",21]
["4.8","Power","15a Plug Assembly, Dedicated Power, Color Red, For Mounting In P801 Metal Skirting","Each",21]
["4.9","Power","Wire, Electrical, Surfex, 2.5 Mm2(Normal Plugs)","P/M",120]
["4.10","Point","Electrical Normal Power Point  complete, excl CB.","Per Point",21]
["4.11","Power","Electrical 2 Pin 5 A Power outlet.","Per Point",1]
["4.12","Power","15a Standard Plugtop","Each",21]
["4.13","Power","15a Plug Assembly, Normal Power,  For Mounting In P801 Metal Skirting","Each",21]
["4.14","Power","Wire, Electrical, Surfex, 2.5 Mm2(Red Plugs)","P/M",120]
["4.15","Infrast","Dual Metal Channel  (Incl Corners, End Caps Etc)","P/M",160]
["4.16","Point","Wifi/APS Connectors","Per Point",1]
[5,null,"Children Library"]
["5.1","Point","UTP CAT6e Data Point complete with flylead and patchlead","Per Point",8]
["5.2","Frame module","45deg ADAPTER PLATE for COMPACT","Each",8]
["5.3","module","RJ 45 WHITE SHUTTER CAT 6 ","Each",8]
["5.4","frame","TRUNKING FRAME 50 x 50","Each",8]
["5.5","Blank blate","25 X 50 BLANK ","Each",8]
["5.6","Point","Electrical Dedicated Power Point  complete, excl CB.","Per Point",8]
["5.7","Power","15a Dedicated Plugtop","Each",8]
["5.8","Power","15a Plug Assembly, Dedicated Power, Color Red, For Mounting In P801 Metal Skirting","Each",8]
["5.9","Power","Wire, Electrical, Surfex, 2.5 Mm2(Normal Plugs)","P/M",90]
["5.10","Point","Electrical Normal Power Point  complete, excl CB.","Per Point",8]
["5.11","Power","15a Standard Plugtop","Each",8]
["5.12","Power","15a Plug Assembly, Normal Power,  For Mounting In P801 Metal Skirting","Each",8]
["5.13","Power","Wire, Electrical, Surfex, 2.5 Mm2","P/M",90]
["5.14","Infrast","Dual Metal Channel  (Incl Corners, End Caps Etc)","P/M",80]
[6,null,"Main Library"]
["6.1","Point","UTP CAT6e Data Point complete with flylead and patchlead","Per Point",10]
["6.2","Frame module","45deg ADAPTER PLATE for COMPACT","Each",10]
["6.3","module","RJ 45 WHITE SHUTTER CAT 6 ","Each",10]
["6.4","frame","TRUNKING FRAME 50 x 50","Each",10]
["6.5","Blank blate","25 X 50 BLANK ","Each",10]
["6.6","Point","Electrical Dedicated Power Point  complete, excl CB.","Per Point",10]
["6.7","Power","15a Dedicated Plugtop","Each",10]
["6.8","Power","15a Plug Assembly, Dedicated Power, Color Red, For Mounting In P801 Metal Skirting","Each",10]
["6.9","Power","Wire, Electrical, Surfex, 2.5 Mm2","P/M",170]
["6.10","Point","Electrical Normal Power Point  complete, excl CB.","Per Point",10]
["6.11","Point","Electrical 2 Pin 5 A Power outlet.","Per Point",2]
["6.12","Power","15a Standard Plugtop","Each",10]
["6.13","Power","15a Plug Assembly, Normal Power,  For Mounting In P801 Metal Skirting","Each",10]
["6.14","Power","Wire, Electrical, Surfex, 2.5 Mm2(Red Plugs)","P/M",170]
["6.15","Infrast","Dual Metal Channel  (Incl Corners, End Caps Etc) Easter Oak","P/M",140]
["6.16","Point","Wifi/APS Connectors","Per Point",1]
[7,null,"Power Requirements"]
[null,null,"SUB DB"]
["7.1","Power","Distribution Cabinet, Surface Mountable, White, 400mm X 300mm X 150mm","Each",1]
["7.2","Power","60a, Earth Leakage, Heineman","Each",1]
["7.3","Power","60a 1 Phase CB/Isolator","Each",1]
["7.4","Power","25a, Circuit Breaker, Heinemann, Std Curve","Each",16]
[8,null,"INFRASTRUCTURE"]
["8.1","Infrast","Nail in Anchors Hilti 6 x 55","Each",100]
["8.2","Infrast","Tape 9mm","Each",6]
["8.3","Infrast","M6  Flat Washer","Each",100]
["8.4","Infrast","Silicone","Each",4]
["8.5","Infrast","BRADY \"0\"  - \"9\" 37/STRIP  BLACK/WHITE","Each",10]
["8.6","Infrast","BRADY \"A\"  - \"Z\" 37/STRIP  BLACK/WHITE","Each",10]
["8.7","Brush panel","BRUSH PANEL SHORT BASE METAL","Each",3]
["8.8","Patch Panel","24 PORT PATCH PANEL CAT 6e LOADED","Each",3]
["8.9","Switch","48 Port Switch","Each",2]
["8.10","Aircon","1800BTU air-conditioner including installation","Each",1]
["8.11","Cabinet","25U Cabinet. (Includes UPS, power surge protection, cabinet management, etc)","Each",1]
[9,null,"Documentation"]
["9.1","Services","UTP testing and labeling","P/P",63]
["9.2","Services","Power Testing and labeling","P/P",126]
["9.3","Services","Cabling Certification","Each",1]
["9.4","Services","Schematic Layout Of Network","P/H",4]

{"sheet":"Oliphantshoek","index":2,"n_rows":46,"n_cols":3,"rows_kept":46}
["Item","Description","QTY"]
[null,"Limpopo LSAC: Oliphantshoek modular LIBRARy"]
[1,"Krone UTP CAT6 Data Point complete with 3m flylead and patchlead",30]
[2,"ADAPTER 22.5 X 45 LEGRAND HK SHUTTER",30]
[{"$f":"A4+1","v":3},"KEYSTONE RJ45 KM8 C6 WHITE STP",30]
[4,"Cover Plate P/O 50x50 E/O",30]
[5,"Collar 50x50",30]
[6,"Euromod Half Blank White",30]
[7,"Surface mount DATA POINT",1]
[8,"Electrical Normal Power Point  complete, excl CB.",30]
[9,"Electrical Dedicated Power Point  complete, excl CB.",30]
[10,"Cover 2 X 4 Vert White 16 Amp",30]
[11,"Cover Socket 2 X 4 Vert Red Ded 16 Amp For MS2",30]
[12,"Plugtop 16 Amp Red",30]
[13,"Cable Surfex 6 X 2 Core + Earth","240M"]
[14,"Dual Metal Channel (Incl Corners, End Caps Etc.) Easter Oak / Hospital Grey","65m"]
[15,"yt2 Surface mount trunking","9m"]
[16,"Switches 48 PORT POE",1]
[17,"Internal Ceiling mount access point",1]
[18,"BRADY \"0\" - \"9\" 37/STRIP BLACK/WHITE",2]
[19,"BRUSH PANEL SHORT BASE METAL",4]
[20,"24 PORT PATCH PANEL CAT 6e LOADED",2]
[21,"15U Cabinet. (Includes UPS, power surge protection, cabinet management, etc.)",1]
[22,"Smart-UPS, 900 Watts /1500 VA, Input 230V /Output 230V, Interface Port USB, Rack mounted",1]
[23,"Distribution Cabinet, Surface Mountable, White, 400mm X 300mm X 150mm",1]
[24,"60a, Earth Leakage",1]
[25,"60a 1 Phase CB/Isolator",1]
[26,"25a, Circuit Breaker, Std Curve",4]
[]
[]
[]
[null,"SUNDRIES/ Infrasrtucture"]
[1,"Tape Brother White 9mm / BRADY \"0\" - \"9\" 37/STRIP BLACK/WHITE",2]
[2,"Insulation Tape - Black",2]
[3,"5mm x 20mm Pop rivets",200]
[4,"M6 Flat Washer",200]
[5,"Silicone",2]
[]
[null,"Documentation"]
[{"$f":"A39+1","v":1},"Test Data Point",31]
[2,"UTP Labelling",62]
[3,"Power Labelling",60]
[4,"Schematic Layout Of Network",3]
[5,"Data Certification",1]
[6,"UTP Test Results",1]
[{"$f":"A44+1","v":6},"COC - Electrical Certification",1]

{"sheet":"Tshitale","index":3,"n_rows":46,"n_cols":3,"rows_kept":46}
["Item","Description","QTY"]
[null,"Limpopo LSAC: Tshitale modular LIBRARy"]
[1,"Krone UTP CAT6 Data Point complete with 3m flylead and patchlead",30]
[2,"ADAPTER 22.5 X 45 LEGRAND HK SHUTTER",30]
[{"$f":"A4+1","v":3},"KEYSTONE RJ45 KM8 C6 WHITE STP",30]
[4,"Cover Plate P/O 50x50 E/O",30]
[5,"Collar 50x50",30]
[6,"Euromod Half Blank White",30]
[7,"Surface mount DATA POINT",1]
[8,"Electrical Normal Power Point  complete, excl CB.",30]
[9,"Electrical Dedicated Power Point  complete, excl CB.",30]
[10,"Cover 2 X 4 Vert White 16 Amp",30]
[11,"Cover Socket 2 X 4 Vert Red Ded 16 Amp For MS2",30]
[12,"Plugtop 16 Amp Red",30]
[13,"Cable Surfex 6 X 2 Core + Earth","240M"]
[14,"Dual Metal Channel (Incl Corners, End Caps Etc.) Easter Oak / Hospital Grey","65m"]
[15,"yt2 Surface mount trunking","9m"]
[16,"Switches 48 PORT POE",1]
[17,"Internal Ceiling mount access point",1]
[18,"BRADY \"0\" - \"9\" 37/STRIP BLACK/WHITE",2]
[19,"BRUSH PANEL SHORT BASE METAL",4]
[20,"24 PORT PATCH PANEL CAT 6e LOADED",2]
[21,"15U Cabinet. (Includes UPS, power surge protection, cabinet management, etc.)",1]
[22,"Smart-UPS, 900 Watts /1500 VA, Input 230V /Output 230V, Interface Port USB, Rack mounted",1]
[23,"Distribution Cabinet, Surface Mountable, White, 400mm X 300mm X 150mm",1]
[24,"60a, Earth Leakage",1]
[25,"60a 1 Phase CB/Isolator",1]
[26,"25a, Circuit Breaker, Std Curve",4]
[]
[]
[]
[null,"SUNDRIES/ Infrasrtucture"]
[1,"Tape Brother White 9mm / BRADY \"0\" - \"9\" 37/STRIP BLACK/WHITE",2]
[2,"Insulation Tape - Black",2]
[3,"5mm x 20mm Pop rivets",200]
[4,"M6 Flat Washer",200]
[5,"Silicone",2]
[]
[null,"Documentation"]
[{"$f":"A39+1","v":1},"Test Data Point",31]
[2,"UTP Labelling",62]
[3,"Power Labelling",60]
[4,"Schematic Layout Of Network",3]
[5,"Data Certification",1]
[6,"UTP Test Results",1]
[{"$f":"A44+1","v":6},"COC - Electrical Certification",1]

{"sheet":"Vuwani","index":4,"n_rows":46,"n_cols":3,"rows_kept":46}
["Item","Description","QTY"]
[null,"Limpopo LSAC: Vuwani modular LIBRARy"]
[1,"Krone UTP CAT6 Data Point complete with 3m flylead and patchlead",30]
[2,"ADAPTER 22.5 X 45 LEGRAND HK SHUTTER",30]
[{"$f":"A4+1","v":3},"KEYSTONE RJ45 KM8 C6 WHITE STP",30]
[4,"Cover Plate P/O 50x50 E/O",30]
[5,"Collar 50x50",30]
[6,"Euromod Half Blank White",30]
[7,"Surface mount DATA POINT",1]
[8,"Electrical Normal Power Point  complete, excl CB.",30]
[9,"Electrical Dedicated Power Point  complete, excl CB.",30]
[10,"Cover 2 X 4 Vert White 16 Amp",30]
[11,"Cover Socket 2 X 4 Vert Red Ded 16 Amp For MS2",30]
[12,"Plugtop 16 Amp Red",30]
[13,"Cable Surfex 6 X 2 Core + Earth","240M"]
[14,"Dual Metal Channel (Incl Corners, End Caps Etc.) Easter Oak / Hospital Grey","65m"]
[15,"yt2 Surface mount trunking","9m"]
[16,"Switches 48 PORT POE",1]
[17,"Internal Ceiling mount access point",1]
[18,"BRADY \"0\" - \"9\" 37/STRIP BLACK/WHITE",2]
[19,"BRUSH PANEL SHORT BASE METAL",4]
[20,"24 PORT PATCH PANEL CAT 6e LOADED",2]
[21,"15U Cabinet. (Includes UPS, power surge protection, cabinet management, etc.)",1]
[22,"Smart-UPS, 900 Watts /1500 VA, Input 230V /Output 230V, Interface Port USB, Rack mounted",1]
[23,"Distribution Cabinet, Surface Mountable, White, 400mm X 300mm X 150mm",1]
[24,"60a, Earth Leakage",1]
[25,"60a 1 Phase CB/Isolator",1]
[26,"25a, Circuit Breaker, Std Curve",4]
[]
[]
[]
[null,"SUNDRIES/ Infrasrtucture"]
[1,"Tape Brother White 9mm / BRADY \"0\" - \"9\" 37/STRIP BLACK/WHITE",2]
[2,"Insulation Tape - Black",2]
[3,"5mm x 20mm Pop rivets",200]
[4,"M6 Flat Washer",200]
[5,"Silicone",2]
[]
[null,"Documentation"]
[{"$f":"A39+1","v":1},"Test Data Point",31]
[2,"UTP Labelling",62]
[3,"Power Labelling",60]
[4,"Schematic Layout Of Network",3]
[5,"Data Certification",1]
[6,"UTP Test Results",1]
[{"$f":"A44+1","v":6},"COC - Electrical Certification",1]