{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["P & G","Supply and Delivery"],"not_rendered":{"external_links":32,"defined_names":1595},"read":"whole","date_system":"1900"}

{"sheet":"P & G","index":0,"n_rows":31,"n_cols":7,"rows_kept":31,"merged":[[5,1,6,1],[5,2,6,2],[5,3,6,3],[5,4,6,4],[5,5,6,5],[5,6,6,6],[30,2,31,2],[30,6,31,6]]}
[]
[null,null," ",{"$nulls":3},"2026-01-05"]
[]
[null,"PROJECT: SUPPLY AND DELIVERY OF GEARBOXES ON AS AND WHEN REQUIRED BASIS AT KUSILE POWER STATION FOR A PERIOD OF FIVE (5) YEARS "]
[]
[null,"ITEM NO.","DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT"]
[]
[]
[null,null,"ITEM 1"]
[null,1,"PRELIMINARIES AND GENERAL"]
[]
[null,1.1,"Safety File","Once Off",{"v":1,"d":"1 "}]
[]
[null,null,"Sub-total Item 1 (Preliminaries and General) carried to Final Summary"]
[]
[null,null,"ITEM 2"]
[null,2,"SUPPLY AND DELIVERY OF GEARBOXES"]
[]
[null,2.1,"Supply and Delivery of Gearboxes","Item",{"v":1,"d":"1 "}]
[]
[null,null,"Sub-total Item 2 (Supply and Delivery of Gearboxes) carried to Final Summary"]
[]
[]
[]
[null,null,"Final Summary"]
[]
[null,"ITEM 1","PRELIMINARIES AND GENERAL"]
[]
[null,"ITEM 2",{"$f":"C17","v":"SUPPLY AND DELIVERY OF GEARBOXES"}]
[]
[null,null,"Final Summary Total (Excl VAT)"]

{"sheet":"Supply and Delivery","index":1,"n_rows":57,"n_cols":9,"rows_kept":57,"merged":[[56,1,56,7]]}
[]
[{"$nulls":8},"2026-01-05"]
[]
[null,"PROJECT: SUPPLY AND DELIVERY OF GEARBOXES ON AS AND WHEN REQUIRED BASIS AT KUSILE POWER STATION FOR A PERIOD OF FIVE (5) YEARS "]
[]
[null,"NO","MATERIAL NUMBER","DESCRIPTION","AREA-LOCATION","UOM","QUANTITY","RATE","AMOUNT"]
[null,1,649044,"GEARBOX: APPLICATION: ASH PLANT; SUPPL P/N: G86-H150B011; LOOPRING; 4072QR10838; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Ash -Plant","EA",4]
[null,2,649043,"GEARBOX: APPLICATION: ASH PLANT; SUPPL P/N: X65-0311514012; AFDICHTRING V BASL 115X140X12; 4072QR10838; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Ash -Plant","EA",4]
[null,3,710056,"GEARBOX: TYPE: 3 STG; RATIO: 191.02:1; SPEED: 1455 RPM; POWER: 5.5 KW; APPLICATION: ASH RECLAIMER MACHINE; SPECIFICATION: KZ148-LA132SP4E- L80GHA; BEVEL HELICON; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Ash -Plant","EA",4]
[null,4,648212,"GEARBOX: TYPE: BALANCE MACHINE; RATIO: 48:1; SPEED: 1392/29 RPM; POWER: 45 KW; SHAFT SIZE: 45K6 MM; APPLICATION: ASH CONDITIONER; ROTATION DIRECTION: CLOCK/ANTI CLOCKWISE; SUPPL P/N: 14226566050/1; SPECIFICATION: HD0-1103LPL1G225; REFERENCE NO: 2FB6301AH10001; MOUNTING: B3; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Ash -Plant","EA",12]
[null,5,649042,"GEARBOX: APPLICATION: ASH PLANT; SUPPL P/N: 268-9RBV10514X; GAMMASEAL 9RB105143055 VIT RVS; 4072QR10838; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Ash -Plant","EA",4]
[null,6,756238,"GEARBOX: TYPE: BEVEL HELICAL; RATIO: 15.96 : 1; SPEED: 94 RPM; POWER: 400 KW; SHAFT SIZE: 80M6 X170 KEYED MM; APPLICATION: ASH CONVEYOR MAIN DRIVE; ROTATION DIRECTION: DUAL OUTPUT SHAFT MULTI DIRECTIONAL; MANUF P/N: X3KR210E/HU/B; DRAWING NO: A04682; INPUT SPEED 1500RPM, OUTPUT SHAFT 195H6 X 283 MM SOLID SHAFT WITHOUT KEYWAY, TYPE OF LUBRICATION SPLASH LUBRICATION.; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Ash -Plant","EA",4]
[null,7,710060,"GEARBOX: TYPE: 3 STG; RATIO: 191.02:1; SPEED: 7.6 RPM; POWER: 5.5 KW; APPLICATION: ASH STACKER MACHINE; SPECIFICATION: KZ148-LA132- ZMP4E-L80-100NM; BEVEL HELICON; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Ash -Plant","EA",4]
[null,8,683105,"GEARBOX: TYPE: PLANETARY RIGHT ANGLE; RATIO: 214:1; SPEED: I/P: 1470 X O/P: 6.87 RPM; POWER: 5.5 KW; SHAFT SIZE: IP 75 H7 X OP 90 H7 MM; APPLICATION: RADIAL STACKER TRAVEL DRIVE; ROTATION DIRECTION: CLOCKWISE AND COUNTER CLOCKWISE; SUPPL P/N: 306-R4-214-FP-P132-B0-G0A; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Ash -Plant","EA",8]
[null,9,649045,"GEARBOX: APPLICATION: ASH PLANT; SUPPL P/N: U65-0319022012; AFDICHTRING BASL 190X220X12; 4072QR10838; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Ash -Plant","EA",4]
[null,10,645223,"GEARBOX: TYPE: SPEED REDUCER; RATIO: 15.5:1; SPEED: I/P 1480; O/P 95.48 RPM; POWER: 365 KW; SHAFT SIZE: I/P DIA 70 X LG 125; O/P DIA 140 X LG 200 MM; APPLICATION: CONVEYOR DRIVE; ROTATION DIRECTION: BI DIRECTIONAL; DRAWING NO: CD00002170REV3 REV 0; MODEL NO: HDD120-2-1SS- LP-D1-VP-B3-FAN-TK; REFERENCE NO: 422635102; DOUBLE OUTPUT; OVERLAND CONVEYORS; BEVEL HELICAL; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Ash -Plant","EA",4]
[null,11,698719,"GEARBOX: TYPE: BEVEL GEAR; RATIO: 3:1; SPEED: 5.6 RPM; POWER: 0.25 KW; APPLICATION: NON RISING SPINDLE GATE VALVE; ROTATION DIRECTION: CLOCKWISE & ANTICLOCKWISE; DRAWING NO: BEVEL GEAR - MOV- 020-ASSY REV 0; REFERENCE NO: B2130812; DIRTY WATER CONTROL VALVE; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMB0756236ER (IF APPLICABLE).","Ash -Plant","EA",12]
[null,12,756236,"GEARBOX: TYPE: BEVEL HELICAL; RATIO: 12.24 : 1; SPEED: 123 RPM; POWER: 75 KW; SHAFT SIZE: 50K6 X 110 KEYED MM; APPLICATION: ASH STACKER MAIN DRIVE; MANUF P/N: X2KR110E/HU/B; DRAWING NO: A04681; INPUT SPEED 1500 RPM, OUTPUT SHAFT 85V6 X131 MM, SOLID SHAFT WITHOUT KEYWAY, TYPE OF LUBRICATION SPLASH LUBRICATION.; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Ash -Plant","EA",4]
[null,13,700696,"GEARBOX: TYPE: BEVEL HELICON THREE STAGE; RATIO: 167.50:1; SPEED: 8.7 K/MIN; POWER: 11 KW; APPLICATION: LIMESTONE STACKER MACHINE; SUPPL P/N: KZ168-LA160-MP4E-L150-GHA; S/N: JHK410 470 1408-624; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Limestone","EA",3]
[null,14,700664,"GEARBOX: TYPE: BEVEL HELICON GEARBOX THREE STAGE; RATIO: 191.02:1; SPEED: 7.6 MIN; POWER: 5.5 KW; APPLICATION: LIMESTONE RECLAIMER MACHINE; SUPPL P/N: KZ148-LA132-SP4E-L80-GHA; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Limestone","EA",3]
[null,15,662538,"GEARBOX: TYPE: PLANETARY; RATIO: 10:1; SPEED: 1.54 RPM; POWER: 0.16 KW; SHAFT SIZE: 18 MM; APPLICATION: LIMESTONE HYDRAULIC FEEDER DRIVE; ROTATION DIRECTION: CLOCKWISE; SUPPL P/N: 2572 00- 02-01; SPECIFICATION: TH-CD-2572-00-02; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Limestone","EA",3]
[null,16,681577,"GEARBOX: TYPE: REDUCTION; RATIO: 11.2:1; SPEED: 1445 RPM; POWER: 20 KW; SHAFT SIZE: 101.5 MM; APPLICATION: COAL STACKER 1 AND 2 - CABLE REEL; ROTATION DIRECTION: CLOCKWISE AND COUNTER CLOCKWISE; SUPPL P/N: 2081624271; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Coal Plant","EA",2]
[null,17,659892,"GEARBOX: TYPE: PLANETARY; RATIO: 1:2; SPEED: 0.57 RPM; POWER: 0.2 KW; SUPPL P/N: MP1- 00013-000-01; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Coal Mobile Feeder","EA",2]
[null,18,703897,"GEARBOX: TYPE: BEVEL HELICAL; RATIO: 715-1; SPEED: 1500 RPM; POWER: 90 KW; APPLICATION: FEEDER 1600; ROTATION DIRECTION: RH; SUPPL P/N: 52- 1561-RH-715-1; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Coal Buffalo Feeder","EA",2]
[null,19,648473,"GEARBOX: TYPE: HELICAL; RATIO: 49.596:1; SPEED: 1480 RPM; POWER: 334 KW; SHAFT SIZE: I/P 60 X O/P 185 MM; APPLICATION: RECLAIMER 1-3 DRUM DRIVE; SUPPL P/N: GB21/TPS- 69; DRAWING NO: 0.84/10342 REV 0; PARALLEL SHAFT: TRIPPLE REDUCTION; DATASHEET SHALL BE SUPPLIED WITH EVERY DELIVERY; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Coal Plant","EA",2]
[null,20,650084,"GEARBOX: TYPE: BEVEL HELICAL GEAR UNIT; SPEED: 12.29-1.64 RPM; APPLICATION: DRIVE COAL FEEDER GEARBOX MILLING PLANT; SUPPL P/N: SP-KUS-F2-05403; SPLASH LUBRICATION; DESIGN: H11; TORQUE: 8007NM; BEARINGS; GEAR TEETH; SEALS; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Coal Plant","EA",2]
[null,21,664364,"GEARBOX: TYPE: SLEW DRIVE 1; RATIO: 1.09; SPEED: 1.61 RPM; POWER: 0.37 KW; SHAFT SIZE: 80 MM; APPLICATION: STACKER HYDRAULIC SYSTEM 0 1EAD30 AE001-MG01; ROTATION DIRECTION: FORWARD/REVERSE; SUPPL P/N: 0973 0 07404-1-10.1; SPECIFICATION: 0973 0 07404-1; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Coal Plant","EA",2]
[null,22,648472,"GEARBOX: TYPE: ANGULAR HELICAL BEVEL; RATIO: 238:1; SPEED: 1440 RPM; POWER: 9.2 KW; APPLICATION: RECLAIMER 1-3 MAIN TRAVEL; ROTATION DIRECTION: BI DIRECTIONAL; SUPPL P/N: GB19/WUV100QL; DRAWING NO: 0.90/51388 REV 0; OUTPUT SHAFT: SOLID SHAFT WITH KEY; 4-STAGES; DATASHEET SHALL BE SUPPLIED WITH EVERY DELIVERY; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Coal Plant","EA",2]
[null,23,629760,"GEARBOX: TYPE: PLANETARY; RATIO: 35:8; SPEED: 350 RPM; POWER: 250 KW; SHAFT SIZE: 280 MM; APPLICATION: FEEDER CONVEYOR FDR-1; ROTATION DIRECTION: MULTITURN; SUPPL P/N: PN319L2.24/5FP.SF.V9AE-A; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Limestone","EA",2]
[null,24,647322,"GEARBOX: TYPE: BEVEL HELICAL; RATIO: 234.6:1; SPEED: 5.05 RPM; POWER: 7.5 KW; APPLICATION: STACKER TRAVEL DRIVE; ROTATION DIRECTION: CLOCK/ANTI CLOCKWISE; SUPPL P/N: GB23/BK90Z-52HR/D13MA4; DATASHEET SHALL BE SUPPLIED WITH EVERY DELIVERY; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Coal Plant","EA",2]
[null,25,645224,"GEARBOX: TYPE: SPEED REDUCER; RATIO: 1.19:5; SPEED: I/P 1480; O/P 75.89 RPM; POWER: 298 KW; SHAFT SIZE: I/P DIA 55 X LG 100; O/P DIA 140 X LG 200 MM; APPLICATION: CONVEYOR DRIVE; ROTATION DIRECTION: BI DIRECTIONAL; DRAWING NO: CD00002171REV03 REV 0; MODEL NO: HD0-120-3-19.S- LP-D1-VP-B3-FAN-TK; REFERENCE NO: 424689601; DOUBLE OUTPUT; APPLICABLE ON TRANSVERSE CONVEYORS; RATED TORQUE: 34750NM; BREATHER: GB16; OUTPUT COUPLING: TC30.330.560 D140/160; INPUT COUPLING REDUCER: TC109H D60D55; TK PIPING KIIS; INPUT COUPLING MOTOR: BR236 \"BLK\" 060D55; BEVEL HELICAL; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Ash -Plant","EA",4]
[null,26,662392,"GEARBOX: TYPE: PLANETARY; RATIO: 100:1; SPEED: 115 RPM; POWER: 11 KW; SHAFT SIZE: 8 MM; APPLICATION:TERRACE CONVEYOR HYDRAULIC DRIVE AND CYLINDER EXTENSION SYSTEM; ROTATION DIRECTION: CLOCKWISE; SUPPL P/N: 2570-00- 03-01; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Coal Plant","EA",2]
[null,27,687606,"GEARBOX: TYPE: BEVEL; RATIO: 10:1; SPEED: 232 RPM; POWER: 2 KW; SHAFT SIZE: DIA 28 MM; APPLICATION: LIMESTONE ST AND ASH RECLAIM; ROTATION DIRECTION: LH/RH; SUPPL P/N: 1691/3; REFERENCE NO: BK50/34V/IEC112/SP; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Limestone","EA",2]
[null,28,664366,"GEARBOX: TYPE: SLEW DRIVE 2; RATIO: 1.18; SPEED: 2 RPM; POWER: 0.45 KW; SHAFT SIZE: 80 MM; APPLICATION: STACKER HYDRAULIC SYSTEM 0 1EAD30 AE002-MG01; ROTATION DIRECTION: FORWARD/REVERSE; SUPPL P/N: 0973 0 07404-1-11.1; SPECIFICATION: 0973 0 07404-1; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Coal Plant","EA",2]
[null,29,661441,"GEARBOX: TYPE: DECLUTCHABLE; RATIO: 104:1; SPEED: 22 RPM; POWER: 1 KW; APPLICATION: GEAR OPERATOR; SPECIFICATION: ILG/D5000-SG600; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Water Treatment Plant","EA",6]
[null,30,661440,"GEARBOX: TYPE: DECLUTCHABLE; RATIO: 68:1; SPEED: 1 RPM; POWER: 0.12 KW; APPLICATION: GEAR OPERATOR; SPECIFICATION: ILG/D2400-SG600; REFERENCE NO: SH784514; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Water Treatment Plant","EA",3]
[null,31,662106,"GEARBOX: TYPE: HELICAL; RATIO: 3.62; SPEED: 1475/408 RPM; POWER: 55 KW; SHAFT SIZE: 90 MM; APPLICATION: PUMP; ROTATION DIRECTION: BI DIRECTIONAL; SPECIFICATION: SK82-IEC250; REFERENCE NO: 2007-37639-100 14421117; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Water Treatment Plant","EA",3]
[null,32,620426,"GEARBOX: TYPE: BEVEL HELICAL; RATIO: 33.88:1; SPEED: 1455/43 RPM; POWER: 30 KW; SHAFT SIZE: 110 MM; APPLICATION: AERATOR; ROTATION DIRECTION: CLOCK/ANTI CLOCKWISE; MODEL NO: ZR168K2S200L4-W; REFERENCE NO: JHK0908-3001588046/3; MOUNTING: V1-1A; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Water Treatment Plant","EA",3]
[null,33,689928,"GEARBOX: TYPE: PARALLEL SHAFT; RATIO: 35.29; SPEED: 41 RPM; POWER: 1.5 KW; APPLICATION: AGITATOR; DRAWING NO: 128D 001 REV 0; REFERENCE NO: FDU1111/2074065 001/2/3; SPECIFICATION: FZAM88B-K4-(90), PLEASE PROVIDE THE FOLLOWING WITH THE GEARBOX: DRAWING, DATA SHEET AND MANUAL; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Water Treatment Plant","EA",3]
[null,34,689922,"GEARBOX: TYPE: HELICAL GEAR; RATIO: 8.92; SPEED: 203 RPM; POWER: 3.3 KW; APPLICATION: AGITATOR; MODEL NO: 2047; REFERENCE NO: C23001/01; INCLUDING MOTOR ADAPTOR TO SUIT EXISTING 0.37KW MOTOR AND MALE FLANGE RIGID COUPLING, PLEASE PROVIDE THE FOLLOWING WITH THE GEARBOX: DRAWING, DATA SHEET AND MANUAL; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Water Treatment Plant","EA",1]
[null,35,690184,"GEARBOX: TYPE: HELICAL GEAR; RATIO: 4.5; SPEED: 77 RPM; POWER: 13.5 KW; APPLICATION: AGITATOR; MANUF P/N: C22883/01; MODEL NO: 2087; INCLUDING MOTOR ADAPTOR TO SUIT EXISTING 3KW MOTOR AND MALE FLANGE RIGID COUPLING, PLEASE PROVIDE THE FOLLOWING WITH THE GEARBOX: DRAWING, DATA SHEET AND MANUAL; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Water Treatment Plant","EA",1]
[null,36,690185,"GEARBOX: TYPE: HELICAL GEAR; RATIO: 12.68; SPEED: 110.4 RPM; POWER: 0.75 KW; APPLICATION: AGITATOR; DRAWING NO: 1.02.4908/9 REV 0; REFERENCE NO: 201018053-100 16951418/9; SPECIFICATION: SK572.1FIEC80, PLEASE PROVIDE THE FOLLOWING WITH THE GEARBOX: DRAWING, DATA SHEET AND MANUAL; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Water Treatment Plant","EA",2]
[null,37,689929,"GEARBOX: TYPE: HELICAL GEAR; RATIO: 3.45; SPEED: 101 RPM; POWER: 7.6 KW; APPLICATION: AGITATOR; MODEL NO: 2077; REFERENCE NO: C22257/02; INCLUDING MOTOR ADAPTOR TO SUIT EXISTING 22KW MOTOR AND MALE FLANGE RIGID COUPLING, PLEASE PROVIDE THE FOLLOWING WITH THE GEARBOX DRAWING, DATA SHEET AND MANUAL; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Water Treatment Plant","EA",2]
[null,38,689904,"GEARBOX: TYPE: HELICAL GEAR; RATIO: 14.18; SPEED: 222 RPM; POWER: 7.8 KW; APPLICATION: AGITATOR; MODEL NO: 2057; REFERENCE NO: C22257/01; INCLUDING MOTOR ADAPTOR TO SUIT EXISTING 0.55 KW MOTOR AND MALE FLANGE RIGIF COUPLING, PLEASE PROVIDE THE FOLLOWING WITH THE GEARBOX: DRAWING, DATA SHEET AND MANUAL; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Water Treatment Plant","EA",1]
[null,39,676747,"GEARBOX: TYPE: PARALLEL SHAFT GEAR UNIT; RATIO: 32.34; SPEED: 44 RPM; POWER: 3 KW; SHAFT SIZE: 60 MM; APPLICATION: DEWATERING AREA SUMP AGITATOR; ROTATION DIRECTION: CLOCKWISE; DRAWING NO: 2024736 0 REV 0; SPECIFICATION: SK4282 VF VL2; REFERENCE NO: 200762844-200; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","FGD","EA",2]
[null,40,676746,"GEARBOX: TYPE: PARALLEL SHAFT GEAR UNIT; RATIO: 45.02; SPEED: 32 RPM; POWER: 7.5 KW; SHAFT SIZE: 80 MM; APPLICATION: BLOWDOWN TANK AGITATOR; ROTATION DIRECTION: CLOCKWISE; SPECIFICATION: SK7282 VF VL2; REFERENCE NO: 200964785-100; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","FGD","EA",2]
[null,41,676745,"GEARBOX: TYPE: PARALLEL SHAFT GEAR UNIT; RATIO: 26.4; SPEED: 54 RPM; POWER: 3 KW; SHAFT SIZE: 80.01 MM; APPLICATION: ABSORBER AREA SUMP AGITATOR; ROTATION DIRECTION: CLOCKWISE; SPECIFICATION: SK4282 VF VL2; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","FGD","EA",6]
[null,42,676750,"GEARBOX: TYPE: PARALLEL SHAFT GEAR UNIT; RATIO: 26.43; SPEED: 54 RPM; POWER: 3 KW; SHAFT SIZE: 80 MM; APPLICATION: REAGENT DISTRIBUTION AREA SUMP AGITATOR; ROTATION DIRECTION: CLOCKWISE; SUPPL P/N: 200762844- 300; SPECIFICATION: SK4282 VF VL2; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","FGD","EA",2]
[null,43,641320,"GEARBOX: TYPE: HELICAL BEVEL GEAR UNIT; RATIO: 13.1; SPEED: 5.1 RPM; POWER: 30 KW; APPLICATION: PANTOGRAPH; ROTATION DIRECTION: BI DIRECTIONAL; SUPPL P/N: A703-UH7013.1 HSB3; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","FGD","EA",2]
[null,44,676751,"GEARBOX: TYPE: PARALLEL SHAFT GEAR UNIT; RATIO: 18.7; SPEED: 78 RPM; POWER: 11 KW; SHAFT SIZE: 100 MM; APPLICATION: REAGENT PREPARATION AREA SUMP AGITATOR; ROTATION DIRECTION: CLOCKWISE; DRAWING NO: 2024735-0 REV 0; SPECIFICATION: SK6282 VF VL2; REFERENCE NO: 2000762844-100; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","FGD","EA",2]
[null,45,713697,"GEARBOX: TYPE: 1/4 TURN; RATIO: 208:1; SPEED: 208 RPM; POWER: 28 KW; SHAFT SIZE: 60 MM; APPLICATION: COMBUSTION DAMPER; ROTATION DIRECTION: CLOCKWISE AND COUNTER CLOCKWISE; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE)","Boiler Milling Plant","EA",6]
[null,46,654592,"GEARBOX: TYPE: PLANETARY BEVEL; SPEED: 990/28.49 RPM; POWER: 920 KW; APPLICATION: COAL MILL; SUPPL P/N: KPV1750S; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Boiler Milling Plant","EA",6]
[null,47,654956,"GEARBOX: TYPE: BEVEL GEAR; SPEED: 1375/3.9 RPM; APPLICATION: DRIVE CLEAN OUT CONVEYOR GEARBOX MILLING; SUPPL P/N: SP-KUS-F2-05032; OUTPUT: 1346NM; DESIGN: H1; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Boiler Milling Plant","EA",6]
[null,48,654830,"GEARBOX: TYPE: WORM; APPLICATION: GATE VALVE PRIMARY AIR MILL 10; 20; 30; 40; 50; SUPPL P/N: GS125.3; HYDRO MECHANICAL TRANSMITION; DIMENSIONS: WD 1910 X LG 2110MM; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Boiler Milling Plant","EA",6]
[null,49,645162,"GEARBOX: TYPE: MILL; SUPPL P/N: SP-KUS-F2-35015; DRAWING NO: B114115-35-03-IG04-00001 REV 0; SPECIFICATION: BG030; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Boiler Milling Plant","EA",6]
[null,50,"N/A","DELIVERY (12 TON CRANE TRUCK)","N/A","PER DAY",60]
[null,"TOTAL EXCL. VAT"]