{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":26,"n_cols":4,"rows_kept":26,"merged":[[2,0,2,1]]}
[]
[]
["MAINTENANCE SIGNIFICANT COMPONENTS "]
["DISCRIPTION"," SPECIFICATION","Components requiring Refurbishment"," Components RFS / Spare"]
["Ejector","Ejector:  IP30 flange mount, spring loaded diaphragm, 100 l/min. rubber seal 230/50x50\nIP30 flange mount, spring loaded diaphragm, 100 l/min. rubber seal 230/50x50",0,0]
["Solenoid Valve"," Solenoid Valve: 24V 10 W 4.5 A, direct acting brass. 3/8 port female, clip /nut lock",0,0]
["Pressure switch","Pressure switch: 24V 10 bar brass,3-pin Farrell, ¼ port",0,0]
["Vacuum switch"," Vacuum switch: 24V ¼ port brass,-100-0 bar 3-pin Farrell adjustable",0,0]
["Vacuum Gauge"," Vacuum Gauge: 2.5 class, G1/4B, -100-0, stop pin on dial. C2 1.2.5",0,0]
["Compressor Pressure switch"," Compressor Pressure switch: MDRP 6-8 bar IP65, 230VV 10A IP 65",0,0]
["Timer switch","Timer switch:  24V IP10 5A Dual Timer, KPE-TR",0,0]
["230v to 24v convertor (UNO)"," 230v to 24v convertor: UNO 100-240V IN, Out 24V 30W 1.25A, class 2. Din rail mount",0,0]
["Change over switch","Change over switch:  Hager SFT125 230V 25A 3.7 KW, din rail mount.",0,0]
["230v to 24v Convertor"," 230v to 24v Convertor: E2000 power supply",0,0]
["Pressure relieve valve"," 230V 9A G1/8 NC, 7W",0,0]
["Auto-drain valve"," 230V NC IP65, 6W 0-16 bar 0-90 minute range",0,0]
["Regulator"," 10 bar max, G3/8 AA class, filter diaphragm, clear glass, top head adjustable",0,0]
["Relay"," 24V IN 250 switching, 6A RIF-O-BPT/2",0,0]
["Timer switch for vacuum pump"," TNN1 Multi-Relay Timer,12-240V 1.6VA,1.1W 3 way setting, 8A din rail mount",0,0]
["Vacuum gauge"," Model 111.12,050mm,-100-0kpa. G1/4 clear glass",0,0]
["Water flushing controller"," SS Base mount, WV-A1,ET-A2. Plastic mechanism",0,0]
["Vacuum sliding rubber gate"," BSV, VAC VALVE KPE-SN-002",0,0]
["Compressor"," 230V 9A single phase 10bar, piston type, oil free B14 Flange, base mount ",7,0]
["Vacuum pump"," 220-230 Single Phase, 0.55 kw 4.7A, SV 1016 C 19M3/h",14,0]
["Blower motor"," 2 pole, 1.08m3/min. single phase 220-230V 1.5KW 9.7A base mount",3,0]
["Water Pump controller"," 220-230V 10A IP65, reset type. 10 bar max",0,0]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0}