{"text_format":"3","workbook":"xlsx","n_sheets":4,"sheets":["0554064","Deviation Schedule","Test Schedule","Eskom Drawing"],"not_rendered":{"images":1,"defined_names":3},"read":"whole","date_system":"1900"}

{"sheet":"0554064","index":0,"n_rows":59,"n_cols":7,"rows_kept":59,"merged":[[0,1,0,6],[1,1,1,6],[2,1,2,6],[3,1,3,6],[5,1,5,6],[6,1,6,6],[9,2,9,3],[10,2,10,3],[11,3,11,4],[19,3,19,4],[28,3,28,4],[32,2,32,4],[33,2,33,4],[34,3,34,4],[36,3,36,4],[38,3,38,4],[46,1,46,6],[47,1,48,6],[49,1,49,6],[51,0,51,6],[53,0,53,1],[58,2,58,3]]}
[null,"ESKOM TENDER E2719DXLIMOU"]
[null,"Technical Schedules A and B for"]
[null," DDT-3074 - CONNECTOR,LUG:AL HORNET 1B M12 45 DEG"]
[null,"NB. SUPPLIERS TO CONFIRM ADHERENCE TO THE LATEST PUBLISHED REVISION OF ALL APPLICABLE ESKOM DRAWINGS"]
[]
[null,"Schedule A:  Purchasers specific requirements"]
[null,"Schedule B:  Guarantees and technical particulars of equipment offered"]
[]
[null,1,null,2,3,4,5]
[null,"Item ","Description",null,"Requirement","Schedule A","Schedule B"]
[null,1,"Product Information"]
[null,1.1,"·","Purchasing details"]
[null,"1.1.1",null,"Eskom SAP No",null,{"v":554064,"d":"0554064"},"xxxxxxxxxx"]
[null,"1.1.2",null,"Manufacturer","Manufacturer name","xxxxxxxxxx"]
[null,"1.1.3",null,"Manufacturer's Product Code","Specify Code","xxxxxxxxxx"]
[null,"1.1.4",null,"Manufacturer's Drawing number & Revision number","Specify No and Rev","xxxxxxxxxx"]
[null,"1.1.5",null,"Manufacturer's physical unique identifier indelibly marked.                                                                    All products must be properly identified by a        durable label that cannot be torn or pulled off for 12 months after purchased to indicate manufacturer, size/stranding of conductor, batch number and catalogue number.\nThe label shall be durable enough to ensure that it remains in place and is legible up to at least 12 months after installation. \n","240-75883110 \n\n\n\n","YES"]
[null,"1.1.6",null,"Knurl marks to indicate the number of crimps required and their position, or the beginning and an end in case of overlapping crimps; and the numbers indicating the sequence of crimps if applicable.","240-75883110 \n\n\n\n","YES"]
[null,"1.1.7",null,"All supplied hardware must be properly identified by a durable paint in the correct colour code that will remain for a minimum of 5 years after purchase and installed outdoors.\n\n","240-75883110 ","YES"]
[null,"1.1.7","·","Compliance to Eskom Buyer's Guide Drawings"]
[null,"1.1.7.1",null,"Filled with jointing compound and capped"," Eskom DDT-3074","YES"]
[null,"1.1.7.2",null,"Conductor diameter ranges"," Eskom DDT-3074","Hornet 16.13 mm","xxxxxxxxxx"]
[null,"1.1.7.3",null,"Palm hole diameter as per SAP number"," Eskom DDT-3074]","1xM12","xxxxxxxxxx"]
[null,"1.1.7.4",null,"Colour code as per SAP number [ 240-75883844]"," Eskom DDT-3074","Red","xxxxxxxxxx"]
[null,"1.1.7.5",null,"Conductor diameter range [ Eskom DDT-3074]","mm","11.0- 17.0"]
[null,"1.1.7.6",null,"Tube inside diameter [ Eskom DDT-3074]","mm","17.0(MAX.)"]
[null,"1.1.7.7",null,"Installation angle of the fitting as per Buyers Guide SAP number  Eskom DDT-3074","Degrees",45,"xxxxxxxxxx"]
[null,"1.1.8",null,"Item sample required, upon request from Eskom  (As per the Technical Criteria Document)","240-75883110 clause 4.9.4","YES","xxxxxxxxxx"]
[null,1.2,"·","Mechanical Properties"]
[null,"1.2.1",null,"Material "," Eskom DDT-3074","Aluminium"]
[null,"1.2.2",null,"Crimping Tool "," Eskom DDT-3074","For use with 4 Point indent crimper ","xxxxxxxxxx"]
[null,"1.2.3",null,"Crimping Force range [240-75883110 ]","kN"," 48 and 55"]
[null,2,"Documentation (to be submitted with tender)"]
[null,null,"Note:  All documentation to also be provided in electronic format."]
[null,2.1,"·","General"]
[null,"2.1.1",null,"Approved Manufacturer Drawings showing markings and dimensions","1 Set submitted","YES"]
[null,2.2,"·","Test Reports",null,"Required"]
[null,"2.2.1",null,"Has the relevant signed mandatory test schedule been submitted.","Signed Test Schedule Submitted ","YES"]
[null,3,null,"Packaging"]
[null,3.1,null,"Tubular compression fittings shall be pre-filled with the jointing compound, capped and placed in a sealed plastic bag.","240-75883110 ","YES"]
[null,3.2,null,"Identical fittings shall be packed together in sealed transparent plastic bags. The thickness of all the plastic material used for plastic bags shall be not less than 100 μm.","240-75883110 ","100 μm"]
[null,3.3,null,"The fittings supplied in large quantities shall be bulk packed in suitable containers. The net weight in each container shall not exceed 30 kg.","240-75883110 ","30kg"]
[null,3.4,null,"On the outside of each container the following information shall be provided:\na) product description;\nb) product code or part number;\nc) name of manufacturer and contact details;\nd) number of components of each type in the container;\ne) address of the destination;\nf) Eskom’s purchase order number;\ng) Eskom’s material SAP number(s).","240-75883110 ","YES"]
[null,3.5,null,"If the product is supplied by a third party supplier (e.g. importers, agents, etc.) the container shall also bear the following information on the outside of the container:\na) name of the supplier / agent\nb) contact details of the supplier / agent","240-75883110 ","YES"]
[null,3.6,null,"Installation instructions provided in packaging",null,"YES"]
[]
[null,"ESKOM TENDER E2719DXLIMOU"]
[null,"Deviations to any of the stated requirements are to be captured on the Deviation Schedule."]
[]
[null,"NB: By signing below the supplier is legally binding themselves to the compliance with the Standard Requirements completed on this Schedule"]
[]
["SUPPLIER SIGNATURES"]
[]
[null,null,"         "]
[{"$nulls":3},"Name (Print)",null,"Company name"]
[]
[]
[]
[null,null,"Sign",null,null,"Date"]

{"sheet":"Deviation Schedule","index":1,"n_rows":48,"n_cols":6,"rows_kept":48,"merged":[[0,0,0,6],[1,0,1,6],[2,0,2,6],[2,7,2,13],[2,14,2,20],[2,21,2,27],[2,28,2,34],[2,35,2,41],[2,42,2,48],[2,49,2,55],[2,56,2,62],[2,63,2,69],[2,70,2,76],[2,77,2,83],[2,84,2,90],[2,91,2,97],[2,98,2,104],[2,105,2,111],[2,112,2,118],[2,119,2,125],[2,126,2,132],[2,133,2,139],[2,140,2,146],[2,147,2,153],[2,154,2,160],[2,161,2,167],[2,168,2,174],[2,175,2,181],[2,182,2,188],[2,189,2,195],[2,196,2,202],[2,203,2,209],[2,210,2,216],[2,217,2,223],[2,224,2,230],[2,231,2,237],[2,238,2,244],[2,245,2,251],[2,252,2,255],[3,0,3,6],[3,7,3,13],[3,14,3,20],[3,21,3,27],[3,28,3,34],[3,35,3,41],[3,42,3,48],[3,49,3,55],[3,56,3,62],[3,63,3,69],[3,70,3,76],[3,77,3,83],[3,84,3,90],[3,91,3,97],[3,98,3,104],[3,105,3,111],[3,112,3,118],[3,119,3,125],[3,126,3,132],[3,133,3,139],[3,140,3,146],[3,147,3,153],[3,154,3,160],[3,161,3,167],[3,168,3,174],[3,175,3,181],[3,182,3,188],[3,189,3,195],[3,196,3,202],[3,203,3,209],[3,210,3,216],[3,217,3,223],[3,224,3,230],[3,231,3,237],[3,238,3,244],[3,245,3,251],[3,252,3,255],[5,0,5,6],[6,2,6,6],[7,2,7,6],[8,2,8,6],[9,2,9,6],[10,2,10,6],[11,2,11,6],[12,2,12,6],[13,2,13,6],[14,2,14,6],[15,2,15,6],[16,2,16,6],[17,2,17,6],[18,2,18,6],[19,2,19,6],[20,2,20,6],[21,2,21,6],[22,2,22,6],[23,2,23,6],[24,2,24,6],[25,2,25,6],[26,2,26,6],[27,2,27,6],[28,2,28,6],[29,2,29,6],[30,2,30,6],[31,2,31,6],[32,2,32,6],[33,2,33,6],[34,2,34,6],[35,2,35,6],[36,2,36,6],[38,0,38,6],[39,0,39,6],[40,0,40,6],[42,0,42,1],[43,2,43,3],[47,2,47,3]]}
["ESKOM TENDER E2719DXLIMOU"]
["Deviation schedule"]
[" DDT-3074 - LUG,ALUMINIUM INDENT CRIMP"]
["SAP No: 0554064 - CONNECTOR,LUG:AL HORNET 1B M12 45 DEG"]
[]
["Any deviations offered to this specification shall be listed below with reasons for deviation.  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective that that specified by Eskom. The deviation must be filled even if there are no deviations.  Post evaluation,  the letter of garantee to confim that the product is not compromised even though it was not tested according to the latest  Standard (240-75883110)."]
["Item","Clause","Description of Deviation"]
{"$rows_empty":31}
["ESKOM TENDER E2719DXLIMOU"]
["NB: By signing below the supplier is legally binding themselves to the compliance with the Standard Requirements completed on this Schedule"]
["SUPPLIER SIGNATURES"]
[]
[null,null,"         "]
[null,null,"Name (Print)",null,null,"Company name"]
[]
[]
[]
[null,null,"Sign",null,null,"Date"]

{"sheet":"Test Schedule","index":2,"n_rows":25,"n_cols":6,"rows_kept":25,"merged":[[0,0,0,6],[1,0,1,6],[2,0,2,6],[3,1,3,5],[4,0,4,6],[14,1,14,5],[16,0,16,6],[17,1,17,7],[20,1,20,2],[24,1,24,2]]}
["ESKOM TENDER E2719DXLIMOU"]
["Test Report Schedule"]
[" DDT-3074 - LUG,ALUMINIUM INDENT CRIMP"]
[null,"The manufacture's test reports are required for the selected SAP number listed on this sheet."]
["SAP No: 0554064 - CONNECTOR,LUG:AL HORNET 1B M12 45 DEG"]
[]
[null,1,2,3,4,5]
[null,"Item ","Description","Standard","Clause No.","Manufacturer's Report No."]
[null,1,"Sampling and visual inspection","240-75883110 ",4.3]
[null,2,"Dimension and material verification ","240-75883110 ",4.4]
[null,3,"Mechanical tension tests","240-75883110 ",4.5]
[null,4,"Heat cycle tests","240-75883110 ",4.6]
[null,5,"Drift Test","240-75883110 ",4.8]
[]
[null,"NB: By signing below the supplier is legally binding themselves to the compliance with the Standard Requirements completed on this Schedule"]
[]
["ESKOM TENDER E2719DXLIMOU"]
[null,"SUPPLIER SIGNATURES"]
[]
[]
[null,"Name (Print)",{"$nulls":3},"Company name"]
[]
[]
[]
[null,"Sign",{"$nulls":3},"Date"]

{"sheet":"Eskom Drawing","index":3,"n_rows":0,"n_cols":0,"rows_kept":0}