{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":45,"n_cols":8,"rows_kept":45}
[]
[]
[]
[null,"ITEM","PAYMENT","DESCRIPTION","UNIT","QUANTITY","  RATE","AMOUNT"]
[null,"NO","REFERS"]
[null,"BROUGHT FORWARD",{"$nulls":5},{"$f":"H1","v":{"v":0,"d":"  0.00"}}]
[]
[{"$nulls":3},"TERRAMESH WALL"]
[null,3,"C12.6 ","MECHANICALLY STABILISED EARTH AND GABIONS"]
[]
[null,3.1,"C12.6.1","Establishment on site for MSE","Sum",1,null,{"$f":"F11*G11","v":{"v":0,"d":"  0.00"}}]
[]
[null,3.2,"C12.6.5","Preparation of surface for laying of geosynthetic","m2",4450,null,{"$f":"F13*G13","v":{"v":0,"d":"  0.00"}}]
[]
[null,3.3,"C12.6.9","Structural geosynthetic reinforcing (LTDS > 110 kN/m longitudinal; > 5 kN/m transverse - Paragrid 200/05 or similar approved) ","m2",39500,null,{"$f":"F15*G15","v":{"v":0,"d":"  0.00"}}]
[]
[null,3.4,"C12.6.11","Backfill (G6 quality material compacted to 95% PROCTOR ) - G6 Materials will be available on site\ndensity","m3",40000,null,{"$f":"F17*G17","v":{"v":0,"d":"  0.00"}}]
[]
[null,3.5,"C12.6.13","Drainage (Refer to dwg. 9368-231 for details)","No",15,null,{"$f":"F19*G19","v":{"v":0,"d":"  0.00"}}]
[]
[null,3.6,"C12.6.14","Foundation trench excavation:"]
[null,null,"C12.6.14.1","Excavating all material situated within the following depth ranges below the surface level"]
[]
[null,3.7,null,"a) 0 m to 1.5 m","m3",4650,null,{"$f":"F24*G24","v":{"v":0,"d":"  0.00"}}]
[]
[null,3.8,"C12.6.15","Surface preparation for bedding the gabions","m3",850,null,{"$f":"F26*G26","v":{"v":0,"d":"  0.00"}}]
[]
[null,3.9,"C12.6.16","Gabions and mattresses:"]
[]
[null,"3.10",null,"Polymer coated galvanised gabion baskets (3 x 1 x 1 m with 2 m \"tail\" - Terramesh or similar approved","m3",1750,null,{"$f":"F30*G30","v":{"v":0,"d":"  0.00"}}]
[]
[null,3.11,"C12.6.17","Needle punched non-woven geotextile (Bidim A4 or similar approved)","m2",6650,null,{"$f":"F32*G32","v":{"v":0,"d":"  0.00"}}]
[]
[{"$nulls":3},"Mechanically Stabilised Earth work must be done in accordance with SANS 8006-1:2018 - Code of practice for strengthened/reinforced soils and other fills and COTO (2020)."]
[]
[]
[]
[]
[]
[]
[null,"TOTAL",{"$nulls":4}," ",{"$f":"IF(SUM(H6:H40)=0,\"\",SUM(H6:H40))","v":""}]
[null,"CONTEGENCIES @10%"]
[]
[null,"VAT @15%"]
[null,"GRAND TOTAL"]