{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Mnaual Valves"],"not_rendered":{"images":1,"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"Mnaual Valves","index":0,"n_rows":13,"n_cols":16,"rows_kept":13,"merged":[[0,0,1,0],[0,1,0,4],[0,5,0,9],[0,10,0,14],[1,1,1,3],[2,0,3,0],[2,1,3,1],[2,2,3,2],[2,3,3,3],[2,4,2,5],[2,6,2,7],[2,8,3,8],[2,9,3,9],[2,10,3,10],[2,11,3,11],[2,12,3,12],[2,13,3,13],[2,14,3,14],[2,15,3,15],[12,1,12,8],[12,12,12,14],[15,1,15,8]]}
[{"$nulls":5}," PTFE Filter Destruction Plant System Valve List\nFor procurement.",{"$nulls":4},"Page 1 of 1"]
[null,"Manual Valves"]
[null,"Valve type ","Valve code","Valve size","Design Conditions",null,"Operating Conditions",null,"Safety Class ","Valve Description","Quantity","NOTES   ","Supplier of Purchase","Lead-time","UNIT PRICING","PRICING"]
[{"$nulls":4},"Temp [°C]","Press.[kPa(g)]","Temp [°C]","Press.[kPa(g)]"]
[1,"Ball Valve ","SB","15 mm",93,1585,30,520,"SC  3","Connection ends: RF, B16.5 or NPT-M/F as B1.20.1, Class 150\nBody: SS, ASTM A182-F316/A351-CF8M\nTrim: 316 SS\nPacking/Seal: Graphite\nBall material: 316 SS\nBonnet/Cap: 316 SS",11]
[2,"Ball Valve ","CB","15 mm",93,1795,"Amb",520,"SC  3","Connection ends: RF, B16.5 or  NPT-M/F as B1.20.1, Class 150\nBody: CS, ASTM A105/A126 WCB\nTrim: CS\nPacking/Seal: Graphite\nBall material: CS\nBonnet/Cap: CS",3]
[3,"Ball Valve ","SB","15 mm",93,20685,"Amb",600,"SC  3","Connection ends: RF, B16.5 or NPT-M/F as B1.20.1, Class 1500\nBody: SS, ASTM A182-F316/A351-CF8M\nTrim: 316 SS\nPacking/Seal: Graphite\nBall material: 316 SS\nBonnet/Cap: 316 SS",15]
[4,"Ball Valve ","SB","15 mm",93,20685,"Amb",20000,"SC  3","Connection ends: RF, B16.5 or  NPT -M/F as B1.20.1, Class 1500\nBody: 316 SS, ASTM A182-F316/A351-CF8M\nTrim: 316 SS\nPacking/Seal: Graphite\nBall material: 316 SS\nBonnet/Cap: 316 SS",1]
[5,"Ball Valve ","CB","25  mm",93,1795,40,520,"SC  3","Connection ends: RF, B16.5 or  NPT-M/F as B1.20.1, Class 150\nBody: CS, ASTM A105/A126 WCB\nTrim: 316 SS\nPacking/Seal: Graphite\nBall material: 316 SS\nBonnet/Cap: 316 SS",3]
[6,"Non-return Valve","SU","15 mm",93,20685,"Amb","600 ","SC  3","Connection ends: RF, B16.5 OR NPT-F/M B1.20.1, Class 1500\nBody: 316 SS, ASTM A182-F316/A351-CF8M\nTrim: 316 SS\nPacking/Seal: API 602\nBall material: 316 SS\nBonnet/Cap: 316 SS",10]
[7,"Non-return Valve","SU","15 mm",93,20685,"Amb",20000,"SC  3","Connection ends: RF, B16.5 OR NPT-F/M B1.20.1, Class 1500\nBody: 316 SS, ASTM A182-F316/A351-CF8M\nTrim: 316 SS\nPacking/Seal: API 602\nBall material: 316 SS\nBonnet/Cap: 316 SS",2]
[8,"Non-return Valve","SU","25 mm",93,1585,45,230,"SC  3","Connection ends: RF, B16.5 OR NPT-F/M B1.20.1, Class 150\nBody: 316 SS, ASTM A182-F316/A351-CF8M\nTrim: 316 SS\nPacking/Seal: API 600\nBall material: 316 SS\nBonnet/Cap: 316 SS",1]
[{"$nulls":9},"Total:",{"$f":"SUM(K5:K12)","v":46},null,"TOTAL:",null,null,{"$f":"SUM( P5:P12)","v":0}]