{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Pricing Schedule"],"not_rendered":{"defined_names":3},"read":"whole","date_system":"1900"}

{"sheet":"Pricing Schedule","index":0,"n_rows":623,"n_cols":9,"rows_kept":623,"merged":[[299,2,299,3]]}
["TENDER: ROC 02 2025/ 26"]
["TENDER FOR THE REPAIR AND MAINTENANCE OF SWIMMING POOLS, AND THE SUPPLY, DELIVERY, REPLACEMENT AND COMMISSIONING "]
["OF ACCESSORIES",{"$nulls":6},"Unit Price x Est. Qty"]
["ITEM","Material Numbers","MATERIAL OR TASK DESCRIPTION","STD REPAIR TASK DESCRIPTION ","UNIT","Estimated Quantity","UNIT PRICE \n(Excluding VAT) \nRATE TO SUPPLY ITEM ONLY OR TO REPLACE/ REPAIR/ SERVICE (Labour and materials included)","TOTAL AMOUNT \n(Excluding VAT) \nRATE TO SUPPLY ITEM ONLY OR TO REPLACE/ REPAIR/ SERVICE (Labour and materials included)"]
["A1",null,"ELECTRIC MOTORS AND PUMPS",null,null,"A","B","AxB=C"]
["A1.1",200000045508,"Motor 3kw 380v 2Pole 6.2-amp complete electric","Supply only new complete motor. ","Per Item",5,"R","R"]
["A1.2",3035093,"Motor 3kw 380v 2Pole 6.2-amp complete electric","Supply and replace with new complete motor.","Per Item",5,"R","R"]
["A1.3",3035094,"Motor 3kw 380v 2Pole 6.2-amp service parts of electric","Service: complete overhaul. Rotor, stator, winding, terminal box and bearings.","Per Item",10,"R","R"]
["A1.4",200000045509,"Motor 3kw 380v 4Pole 6.9-amp complete electric","Supply only new complete motor.","Per Item",5,"R","R"]
["A1.5",3035095,"Motor 3kw 380v 4Pole 6.9-amp complete electric","Supply and replace with new complete motor.","Per Item",5,"R","R"]
["A1.6",3035096,"Motor 3kw 380v 4Pole 6.9-amp service parts on electric ","Service: complete overhaul. Rotor, stator, winding, terminal box and bearings.","Per Item",10,"R","R"]
["A1.7",200000045510,"Motor 4kw 380v 2Pole 8,2-amp complete electric","Supply only new complete motor.","Per Item",5,"R","R"]
["A1.8",3035097,"Motor 4kw 380v 2Pole 8.2-amp complete electric","Supply and replace new complete motor.","Per Item",5,"R","R"]
["A1.9",3035098,"Motor 4kw 380v 2Pole 8.2-amp service parts on electric","Service: complete overhaul. Rotor, stator, winding, terminal box and bearings.","Per Item",10,"R","R"]
["A1.10",200000045511,"Motor 4kw 380v 4Pole 9-amp complete electric","Supply only new complete motor.","Per Item",5,"R","R"]
["A1.11",3035099,"Motor 4kw 380v 4Pole 9-amp complete electric","Supply and replace new complete motor.","Per Item",5,"R","R"]
["A1.12",3035100,"Motor 4kw 380v 4Pole 9-amp service parts on electric","Service:  complete overhaul. Rotor, stator, winding, terminal box and bearings.","Per Item",10,"R","R"]
["A1.13",200000045512,"Motor 5.5kw 380v 4Pole 11-amp complete electric","Supply only new complete motor.","Per Item",5,"R","R"]
["A1.14",3035101,"Motor 5.5kw 380v 4Pole 11-amp complete electric","Supply and replace new complete motor.","Per Item",5,"R","R"]
["A1.15",3035102,"Motor 5.5kw 380v, 4Pole 11-amp service parts on electric","Service: complete overhaul. Rotor, stator, winding, terminal box and bearings.","Per Item",10,"R","R"]
["A1.16",200000045513,"Motor 7,5kw 380v 4Pole 15-amp complete electric","Supply only new complete motor.","Per Item",5,"R","R"]
["A1.17",3035103,"Motor 7,5kw 380v 4Pole 15-amp complete electric","Supply and replace new complete motor.","Per Item",5,"R","R"]
["A1.18",3035104,"Motor 7.5kw 380v, 4Pole 15-amp service parts on electric","Service: complete overhaul. Rotor, stator, winding, terminal box and bearings.","Per Item",10,"R","R"]
["A1.19",200000045514,"Motor 11kw 380v 4Pole 21-amp complete electric","Supply only new complete motor.","Per Item",5,"R","R"]
["A1.20",3035105,"Motor 11kw 380v 4Pole 21-amp complete electric","Supply and replace new complete motor.","Per Item",5,"R","R"]
["A1.21",3035106,"Motor 11kw 380v, 4Pole 21-amp service parts on electric","Service: complete overhaul. Rotor, stator, winding, terminal box and bearings.","Per Item",10,"R","R"]
["A1.22",200000045515,"Motor 15kw 380v 4Pole 28-amp complete electric","Supply only new complete motor.","Per Item",5,"R","R"]
["A1.23",3035107,"Motor 15kw 380v 4Pole 28-amp complete electric","Supply and replace new complete motor.","Per Item",5,"R","R"]
["A1.24",3035108,"Motor 15kw 380v 4Pole 28-amp service parts on electric","Service: complete overhaul. Rotor, stator, winding, terminal box and bearings.","Per Item",10,"R","R"]
["A1.25",200000045516,"Motor 18,5kw 380v 4Pole 35.5-amp complete electric","Supply only new complete motor.","Per Item",10,"R","R"]
["A1.26",3036480,"Motor 18,5kw 380v 4Pole 35,5-amp complete electric","Supply and replace new complete motor.","Per Item",10,"R","R"]
["A1.27",3035109,"Motor 18,5kw 380v 4Pole 35,5-amp service parts on electric","Service: complete overhaul. Rotor, stator, winding, terminal box and bearings.","Per Item",20,"R","R"]
["A1.28",200000045517,"Motor 30kw 380v 4Pole 54.7-amp complete electric","Supply only new complete motor.","Per Item",1,"R","R"]
["A1.29",3035110,"Motor 30kw 380v 4Pole 54.7-amp complete electric","Supply and replace new complete motor.","Per Item",1,"R","R"]
["A1.30",3035111,"Motor 30kw 380v 4Pole 54.7-amp service parts on electric","Service: complete overhaul. Rotor, stator, winding, terminal box and bearings.","Per Item",2,"R","R"]
["A1.31",200000045518,"Waste Water submersible pump complete    1.1kw 220v with float level control          ","Supply only new complete motor Operating Conditions. Refer to 3.1 Specification details","Per Item",10,"R","R"]
["A1.32",200000045519,"Layflat Hose for Wastewater pump","Supply only new complete 50mm Layflat Hose 4 bar.","Per meter",10,"R","R"]
["A2",null,"SERVICE PARTS ON PUMPS"]
["A2.1",3035114,"Pump. Flow rate 60 m³/h @ 10m head - service parts","Service: All bearings and seals. The mechanical seal. Changing the bushings and shafts. O-rings and impellers.","Per Item",5,"R","R"]
["A2.2",3035115,"Pump. Flow rate 70 m³/h @ 10m - service parts","Service: All bearings and seals. The mechanical seal. Changing the bushings and shafts. O-rings and impellers.","Per Item",5,"R","R"]
["A2.3",3035116,"Pump. Flow rate 80 m³/h @ 10m - service parts","Service: All bearings and seals. The mechanical seal. Changing the bushings and shafts. O-rings and impellers.","Per Item",5,"R","R"]
["A2.4",3035117,"Pump. Flow rate 125 m³/h @ 10m - service parts","Service: All bearings and seals. The mechanical seal. Changing the bushings and shafts. O-rings and impellers.","Per Item",5,"R","R"]
["A2.5",3035112,"Pump. Flow rate 250 m³/h @ 11m - service parts","Service: All bearings and seals. The mechanical seal. Changing the bushings and shafts. O-rings and impellers.","Per Item",2,"R","R"]
["A2.6",3035113,"Pump. Flow rate 360 m³/h @ 10m - service parts","Service: All bearings and seals. The mechanical seal. Changing the bushings and shafts. O-rings and impellers.","Per Item",1,"R","R"]
["A2.7",3035120,"Rubber coupling F100","Supply and replace rubber coupling providing flexibility and supporting the misalignment of motor shafts between motors and pump.","Per Item",20,"R","R"]
["A2.8",3035118,"Tyre up to F120 ","Supply and replace rubber coupling providing flexibility and supporting the misalignment of motor shafts between motors and pump.","Per Item",20,"R","R"]
["A2.9",200000044965,"Spanner 3-Way","Supply only Industrial Filtration pump lid spanner 3-Way PVC Industrial Filtration pump lid spanner up to 5,5 kw up to 5,5 kw.","Per Item",20,"R","R"]
["A2.10",200000045520,"Spanner crescent","Supply only Industrial Filtration pump lid spanner crescent shaped PVC Industrial Filtration pump lid spanner up to 5,5 kw up to 5,5 kw.","Per Item",20,"R","R"]
["A2.11",200000044966,"Basket strainer ","Supply only Industrial Filtration pump basket strainer PVC Industrial Filtration pump up to 5,5 kw up to 5,5 kw.","Per Item",20,"R","R"]
["A3",null,"COMPLETE ELECTRICAL MOTORS AND PUMPS"]
["A3.1",200000045521,"Motor with pump 3kw 380v 2Pole 6.2-amp electric motor. Pump flow rate 70m³/h @ 10m - complete","Supply only - new complete motor with pump.","Per Item",2,"R","R"]
["A3.2",3035119,"Motor with pump 3kw 380v 2Pole 6.2-amp electric motor. Pump flow rate 70m³/h @ 10m - complete","Supply and replace with new complete motor with pump.","Per Item",1,"R","R"]
["A3.3",200000045522,"Motor with pump 4kw 380v 2Pole 8.2-amp electric motor. Pump flow rate 60m³/h @ 10m - complete","Supply only - new complete motor with pump.","Per Item",2,"R","R"]
["A3.4",3035121,"Motor with pump 4kw 380v 2Pole 8.2-amp electric motor. Pump flow rate 60 m³/h @ 10m - complete","Supply and replace with new complete motor with pump.","Per Item",1,"R","R"]
["A3.5",200000045523,"Motor with pump 4kw 380v 4Pole 9-amp electric motor.  Pump flow rate 80 m³/h @ 10m - complete","Supply only - new complete motor with pump.","Per Item",2,"R","R"]
["A3.6",3035122,"Motor with pump 4kw 380v 4Pole 9-amp electric motor.  Pump flow rate 80 m³/h @ 10m - complete","Supply and replace with new complete motor with pump.","Per Item",1,"R","R"]
["A3.7",200000045524,"Motor & pump 5.5kw 380v 4 Pole 11amp. Flow rate 125m³/h @ 10m - complete","Supply only - new complete motor with pump.","Per Item",2,"R","R"]
["A3.8",3035123,"Motor & pump 5.5kw 380v 4 Pole 11amp. Flow rate 125m³/h @ 10m - complete","Supply and replace with new complete motor with pump.","Per Item",1,"R","R"]
["A3.9",200000045525,"Motor & pump 11kw 380v 4 Pole 21amp. Flow rate 150m³/h @ 10m - complete","Supply only - new complete motor with pump.","Per Item",2,"R","R"]
["A3.10",3035124,"Motor & pump 11kw 380v 4 Pole 21amp. Flow rate 150m³/h @ 10m - complete","Supply and replace with new complete motor with pump.","Per Item",1,"R","R"]
["A3.11",200000045526,"Motor & pump 15kw 380v 4 Pole 28amp. Flow 250rate m³/h @ 10m - complete","Supply only - new complete motor with pump.","Per Item",2,"R","R"]
["A3.12",3035125,"Motor & pump 15kw 380v 4 Pole 28amp. Flow 250rate m³/h @ 10m - complete","Supply and replace with new complete motor with pump.","Per Item",1,"R","R"]
["A3.13",200000045527,"Motor & pump 22kw 380v 4 Pole 43amp. Flow rate 360m³/h @ 10m - complete","Supply only - new complete motor with pump.","Per Item",2,"R","R"]
["A3.14",3036351,"Motor & pump 22kw 380v 4 Pole 43amp. Flow rate 360m³/h @ 10m - complete","Supply and replace with new complete motor with pump.","Per Item",1,"R","R"]
["A4",null,"BOOSTER AND SUMP PUMPS"]
["A4.1",200000045528,"Chlorine booster pump 0.75kw 230v 4.7 amps, 2400rpm. Flow rate 2.5 m³/h @ 15m head - complete ","Supply only new complete motor with pump.","Per Item",3,"R","R"]
["A4.2",3035126,"Chlorine booster pump 0.75kw 230v 4.7 amps, 2400rpm. Flow rate 2.5 m³/h @ 15m head - complete ","Supply and replace with new complete motor with pump.","Per Item",2,"R","R"]
["A4.3",200000045529,"Stainless steel sump pump with float switch and automatic level control 0.25kw 230v 2pole 1.9 amp. Flow rate 20 150L/min 1,5m - 7m head - complete ","Supply only new complete motor with pump.","Per Item",3,"R","R"]
["A4.4",3035127,"Stainless steel sump pump with float switch and automatic level control 0.25kw 230v 2pole 1.9 amp. Flow rate 20 150L/min 1,5m - 7m head - complete ","Supply and replace with new complete motor with pump.","Per Item",2,"R","R"]
["A4.5",200000045530,"Filtration pump 1.1kw 230v 7.1 amps, Flow rate 18 m³/h @ 15m head - complete ","Supply only new complete motor with pump.","Per Item",3,"R","R"]
["A4.6",3035129,"Filtration pump 1.1kw 230v 7.1 amps, Flow rate 18 m³/h @ 15m head - complete ","Supply and replace with new complete motor with pump.","Per Item",2,"R","R"]
["A4.7",200000045531,"Filtration pump 1.5kw 230v 9.8 amps, Flow rate 27 m³/h @ 15m head - complete ","Supply only new complete motor with pump.","Per Item",3,"R","R"]
["A4.8",3035130,"Filtration pump 1.5kw 230v 9.8 amps, Flow rate 27 m³/h @ 15m head - complete ","Supply and replace with new complete motor with pump.","Per Item",2,"R","R"]
["A4.9",200000045532,"Filtration pump 0.75kw 230V 4.4 amps. Flow rate 14 m³/h - complete ","Supply only new complete motor with pump.","Per Item",3,"R","R"]
["A4.10",3035128,"Filtration pump 0.75kw 230V 4.4 amps. Flow rate 14 m³/h - complete ","Supply and replace with new complete motor with pump.","Per Item",2,"R","R"]
["A4.11",200000045533,"Water plant Booster Pump 0,75kw 230volt ","Supply only new complete motor with pump.","Per Item",4,"R","R"]
["A4.12",3035131,"Water plant Booster Pump 0,75kw 230volt","Supply and replace with new complete motor with pump.","Per Item",4,"R","R"]
["A4.13",200000045535,"Water plant Booster Pump 1,1kw 230volt","Supply only new complete motor with pump.","Per Item",3,"R","R"]
["A4.14",3035132,"Water plant Booster Pump 1,1kw 230volt","Supply and replace with new complete motor with pump.","Per Item",3,"R","R"]
["A4.15",200000045534,"Water plant Booster Pump 1,5kw 230volt","Supply only new complete motor with pump.","Per Item",2,"R","R"]
["A4.16",3035133,"Water plant Booster Pump 1,5kw 230volt","Supply and replace with new complete motor with pump.","Per Item",2,"R","R"]
["A4.17",200000045536,"Electronic Pump Control new complete up to 10bar, max 10amps, 220volt","Supply only new complete motor with pump.","Per Item",5,"R","R"]
["A4.18",3035134,"Electronic Pump Control new complete up to 10bar, max 10amps, 220volt","Supply and replace with new complete motor with pump.","Per Item",5,"R","R"]
["Total for Category A (Excluding VAT)",{"$nulls":6},"R"]
[]
["B1",null,"ELECTRICAL ACCESSORIES AND CABLES"]
["B1.1",3035135,"Digital timers for pumps","Supply and replace large LCD display with real time display. Refer to 3.1 Specification details","Per Item",10,"R","R"]
["B1.2",3035136,"Float switches","Supply and replace Float switch with a liquid level regulator. Liquid density between 0.95 and 1.10g/cm³.","Per Item",10,"R","R"]
["B1.3",3035137,"DB box new complete ","Supply and replace DB Box IP65 Waterproof. With a neutral/ earth bar and circuit breakers without transformer.","Per Item",5,"R","R"]
["B1.4",3035138,"DB Box enclosure","Supply and replace DB Box Steel enclosure only. IP55 300mmx250mmx200mm.","Per Item",5,"R","R"]
["B1.5",3035139,"Transformers","Supply and replace new complete with end covers and terminal blocks Input Voltage: 100-240V AC 50/60Hz. Output voltage: 12VDC.","Per Item",20,"R","R"]
["B2",null,"STARTERS"]
["B2.1",3035140,"Starter 5.5-8 amp","Supply and replace starter (direct online) 5.5-8 amp, single phase - complete electric.","Per Item",10,"R","R"]
["B2.2",3035141,"Starter 7-10 amp","Supply and replace starter (direct online) 7-10 amp, 3 phase - complete electric.","Per Item",10,"R","R"]
["B2.3",3035142,"Starter 9-13 amp","Supply and replace starter (direct online) 9-13 amp, 3 phase - complete electric.","Per Item",10,"R","R"]
["B2.4",3035143,"Star/Delta starter 16-24 amp","Supply and replace star/delta starter 16–24 amp overload, 3 phase - complete electric.","Per Item",2,"R","R"]
["B2.5",3035144,"Star/Delta starter 28-36 amp","Supply and replace star/delta starter 28-36 amp overload, 3 phase - complete electric.","Per Item",2,"R","R"]
["B3",null,"CONTACTORS"]
["B3.1",3035145,"Electrical Contactors","Supply and replace contactor 9A 3Pole 4Kw 400V.","Per Item",10,"R","R"]
["B3.2",3035146,"Electrical Contactors","Supply and replace contactor 25A 3Pole 11Kw 230V.","Per Item",10,"R","R"]
["B3.3",3035147,"Electrical Contactors","Supply and replace contactor 40A 3Pole 18.5Kw 230V.","Per Item",10,"R","R"]
["B3.4",3035148,"Electrical Contactors","Supply and replace contactor 65A 3Pole 30Kw 230V.","Per Item",10,"R","R"]
["B4",null,"BREAKERS AND ISOLATORS"]
["B4.1",3035149,"Weatherproof isolator","Supply and replace IP56 surface mount, single pole 15amp.","per item",10,"R","R"]
["B4.2",3035150,"Weatherproof isolator","Supply and replace IP56 surface mount, single pole 20amp.","Per Item",10,"R","R"]
["B4.3",3035151,"Weatherproof isolator","Supply and replace IP56 surface mount, single pole 30amp.","Per Item",10,"R","R"]
["B4.4",3035152,"Weatherproof isolator","Supply and replace IP56 surface mount, triple pole 20amp.","Per Item",10,"R","R"]
["B4.5",3035153,"Weatherproof isolator","Supply and replace IP56 surface mount, triple pole 35amp.","Per Item",10,"R","R"]
["B4.6",3035154,"Circuit breaker","Supply and replace 220v 6ka 15-amp, single pole.","Per Item",15,"R","R"]
["B4.7",3035155,"Circuit breaker","Supply and replace 220v 6ka 20-amp, single pole.","Per Item",15,"R","R"]
["B4.8",3035156,"Circuit breaker","Supply and replace 220v 6ka 30-amp, single pole.","Per Item",15,"R","R"]
["B4.9",3035157,"Circuit breaker","Supply and replace 400v 6ka 20-amp, triple pole.","Per Item",15,"R","R"]
["B4.10",3035158,"Circuit breaker","Supply and replace 400v 6ka 35-amp, triple pole.","Per Item",15,"R","R"]
["B4.11",3035159,"Circuit breaker","Supply and replace 400v 6ka 60-amp, triple pole.","Per Item",15,"R","R"]
["B4.12",3035160,"Compression gland","Supply and replace Nr 0 PVC compression.","Per Item",25,"R","R"]
["B4.13",3035161,"Steel cable gland","Supply and replace Nr 1 Steel armed cable gland.","Per Item",10,"R","R"]
["B4.14",3035162,"Steel cable gland","Supply and replace Nr 2 Steel armed cable gland.","Per Item",10,"R","R"]
["B5",null,"ELECTRICAL CABLES"]
["B5.1",3035163,"Trailing Cable","Supply and replace 2.5mm 3 core.","Per meter",20,"R","R"]
["B5.2",3035164,"Trailing Cable","Supply and replace 2.5mm 4 core.","Per meter",20,"R","R"]
["B5.3",3035165,"Trailing Cable","Supply and replace 4mm 3 core.","Per meter",20,"R","R"]
["B5.4",3035166,"Trailing Cable","Supply and replace 4mm 4 core.","Per meter",20,"R","R"]
["B5.5",3035167,"Trailing Cable","Supply and replace 6mm 3 core.","Per meter",20,"R","R"]
["B5.6",3035168,"Trailing Cable","Supply and replace 6mm 4 core.","Per meter",20,"R","R"]
["B5.7",3035169,"Trailing Cable","Supply and replace 10mm 4 core.","Per meter",20,"R","R"]
["B5.8",3035170,"Trailing Cable","Supply and replace 16mm 4 core.","Per meter",20,"R","R"]
["B5.9",3035177,"Power Cable Splice Kit (Pourable resin sealing compound, funnels & end sealing strips). 82-A1 Conductor Size #2 AWG (max.). Connector OD 13/32\" (max.). Cable OD 5/8\" (max.). Sheath Opening (L) 4 1/2\" (max.) (A) ½ Connector Length (B) ¼”.","Supply and replace with inline splices on unshielded synthetic insulated cables (max 5kV) & multiple conductor cables (max 1kV used with UL submerged connectors up to 600 volts & 90°C.","Per item",10,"R","R"]
["B5.10",3035178,"Power Cable Splice Kit (Pourable resin sealing compound, funnels & end sealing strips). 82-A2 Conductor Size #2 AWG (min.) #3/0 AWG (max.). Connector OD 5/8\" (max.). Cable OD 1\" (max.). Sheath Opening (L) 6\" (max.) (A) ½ Connector Length (B) ½\".","Supply and replace with inline splices on unshielded synthetic insulated cables (max 5kV) & multiple conductor cables (max 1kV used with UL submerged connectors up to 600 volts & 90°C.","Per item",10,"R","R"]
["B5.11",3036363,"Power Cable Splice Kit (Pourable resin sealing compound, funnels & end sealing strips). 82-A3 Conductor Size #3/0 (min.) 200 kcmil (max.). Connector OD 1\" (max.). Cable OD 1 9/16\" (max.). Sheath Opening (L) 9\" (max.). (A) ½ Connector Length (B) ½\".","Supply and replace with inline splices on unshielded synthetic insulated cables (max 5kV) & multiple conductor cables (max 1kV used with UL submerged connectors up to 600 volts & 90°C.","Per item",10,"R","R"]
["B5.12",3036365,"Submersible Cable 2,5 4 core","Supply only Submersible Cable 2,5 4 core.","Per meter",10,"R","R"]
["B5.13",3036366,"Submersible Cable 4.0 4 core","Supply only Submersible Cable 4.0 4 core.","Per meter",10,"R","R"]
["Total for Category B (Excluding VAT)",{"$nulls":6},"R"]
[]
["C1",null,"PIPES, FITTINGS AND VALVES"]
["C1.1",3035179,"UPVC piping class 6","Supply and replace 250mm UPVC Pipe.","Per meter",200,"R","R"]
["C1.2",3036487,"UPVC piping class 6","Supply and replace 200mm UPVC Pipe.","Per meter",200,"R","R"]
["C1.3",3036486,"UPVC piping class 6","Supply and replace 160mm UPVC Pipe.","Per meter",200,"R","R"]
["C1.4",3036485,"UPVC piping class 6","Supply and replace 110mm UPVC Pipe.","Per meter",200,"R","R"]
["C1.5",3036484,"UPVC piping class 6","Supply and replace 90mm UPVC Pipe.","Per meter",200,"R","R"]
["C1.6",3036483,"UPVC piping class 6","Supply and replace 75mm UPVC Pipe.","Per meter",200,"R","R"]
["C1.7",3036482,"UPVC piping class 6","Supply and replace 63mm UPVC Pipe.","Per meter",200,"R","R"]
["C1.8",3036481,"UPVC piping class 6","Supply and replace 50mm UPVC Pipe.","Per meter",200,"R","R"]
["C1.9",3036498,"UPVC piping class 16","Supply and replace 25mm UPVC Pipe.","Per meter",100,"R","R"]
["C1.10",3036497,"UPVC piping class 16","Supply and replace 20mm UPVC Pipe.","Per meter",100,"R","R"]
["C1.11",3036496,"UPVC piping class 12","Supply and replace 250mm UPVC Pipe.","Per meter",10,"R","R"]
["C1.12",3036495,"UPVC piping class 12","Supply and replace 200mm UPVC Pipe.","Per meter",10,"R","R"]
["C1.13",3036494,"UPVC piping class 12","Supply and replace 160mm UPVC Pipe.","Per meter",10,"R","R"]
["C1.14",3036493,"UPVC piping class 12","Supply and replace 110mm UPVC Pipe.","Per meter",10,"R","R"]
["C1.15",3036492,"UPVC piping class 12","Supply and replace 90mm UPVC Pipe.","Per meter",10,"R","R"]
["C1.16",3036491,"UPVC piping class 12","Supply and replace 75mm UPVC Pipe.","Per meter",10,"R","R"]
["C1.17",3036490,"UPVC piping class 12","Supply and replace 63mm UPVC Pipe.","Per meter",10,"R","R"]
["C1.18",3036489,"UPVC piping class 12","Supply and replace 50mm UPVC Pipe.","Per meter",10,"R","R"]
["C1.19",3036488,"UPVC piping class 12","Supply and replace 25mm UPVC Pipe.","Per meter",10,"R","R"]
["C2",null,"ELBOWS AND ADAPTERS"]
["C2.1",3036499,"PVC male adapter 50mm class 12","Supply and replace 50mm PVC.","Per item",100,"R","R"]
["C2.2",3036519,"PVC non return 50mm plc. double union class 12","Supply and replace 50mm PVC.","Per item",100,"R","R"]
["C2.3",3036518,"Elbows 90° PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 250mm PVC.","Per item",25,"R","R"]
["C2.4",3036517,"Elbows 90° PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 200mm PVC.","Per item",25,"R","R"]
["C2.5",3036516,"Elbows 90° PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 160mm PVC.","Per item",25,"R","R"]
["C2.6",3036515,"Elbows 90° PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 110mm PVC.","Per item",25,"R","R"]
["C2.7",3036514,"Elbows 90° PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 90mm PVC.","Per item",25,"R","R"]
["C2.8",3036513,"Elbows 90° PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 75mm PVC.","Per item",25,"R","R"]
["C2.9",3036512,"Elbows 90° PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 63mm PVC.","Per item",25,"R","R"]
["C2.10",3036511,"Elbows 90° PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 50mm PVC.","Per item",25,"R","R"]
["C2.11",3036510,"Elbows 90° PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 25mm PVC.","Per item",25,"R","R"]
["C2.12",3036509,"Elbows 90° PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 20mm PVC.","Per item",25,"R","R"]
["C2.13",3036508,"Elbows 45° PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 250mm PVC.","Per item",25,"R","R"]
["C2.14",3036507,"Elbows 45° PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 200mm PVC.","Per item",25,"R","R"]
["C2.15",3036506,"Elbows 45° PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 160mm PVC.","Per item",25,"R","R"]
["C2.16",3036505,"Elbows 45° PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 110mm PVC.","Per item",25,"R","R"]
["C2.17",3036504,"Elbows 45° PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 90mm PVC.","Per item",25,"R","R"]
["C2.18",3036503,"Elbows 45° PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 75mm PVC.","Per item",25,"R","R"]
["C2.19",3036502,"Elbows 45° PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 63mm PVC.","Per item",25,"R","R"]
["C2.20",3036501,"Elbows 45° PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 50mm PVC.","Per item",25,"R","R"]
["C2.21",3036500,"Elbows 45° PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 25mm PVC.","Per item",25,"R","R"]
["C2.22",3035180,"Elbows 45° PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 20mm PVC.","Per item",25,"R","R"]
["C3",null,"COUPLINGS"]
["C3.1",3036528,"Couplings PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 250mm PVC.","Per item",10,"R","R"]
["C3.2",3036527,"Couplings PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 200mm PVC.","Per item",10,"R","R"]
["C3.3",3036526,"Couplings PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 160mm PVC.","Per item",10,"R","R"]
["C3.4",3036525,"Couplings PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 110mm PVC.","Per item",10,"R","R"]
["C3.5",3036524,"Couplings PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 90mm PVC.","Per item",10,"R","R"]
["C3.6",3036523,"Couplings PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 75mm PVC.","Per item",10,"R","R"]
["C3.7",3036522,"Couplings PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 63mm PVC.","Per item",10,"R","R"]
["C3.8",3036521,"Couplings PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 50mm PVC.","Per item",10,"R","R"]
["C3.9",3036520,"Couplings PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 25mm PVC.","Per item",10,"R","R"]
["C3.10",3035181,"Couplings PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 20mm PVC.","Per item",10,"R","R"]
["C3.11",3035171,"Repair coupling Ranger Cast Iron High Pressure Piping","Supply and replace 90mm (PN 16).","Per item",3,"R","R"]
["C3.12",3035172,"Repair coupling Ranger Cast Iron High Pressure Piping","Supply and replace 150mm (PN 16).","Per item",3,"R","R"]
["C3.13",3035173,"Repair coupling Ranger Cast Iron High Pressure Piping","Supply and replace 200mm (PN 16).","Per item",4,"R","R"]
["C3.14",3036367,"Quick release (Polypropylene black plastic)","Supply and replace female bsp adaptor 65mm.","Per item",10,"R","R"]
["C3.15",3036368,"Quick release (Polypropylene black plastic)","Supply and replace female bsp adaptor 80mm.","Per item",10,"R","R"]
["C3.16",3036369,"Quick release (Polypropylene black plastic)","Supply and replace hose tail coupler 65mm.","Per item",10,"R","R"]
["C3.17",3036370,"Quick release (Polypropylene black plastic)","Supply and replace hose tail coupler 80mm.","Per item",10,"R","R"]
["C4",null,"JOINTS"]
["C4.1",3036537,"T/Joints PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 250mm PVC.","Per item",10,"R","R"]
["C4.2",3036536,"T/Joints PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 200mm PVC.","Per item",10,"R","R"]
["C4.3",3036535,"T/Joints PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 160mm PVC.","Per item",10,"R","R"]
["C4.4",3036534,"T/Joints PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 110mm PVC.","Per item",25,"R","R"]
["C4.5",3036533,"T/Joints PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 90mm PVC.","Per item",25,"R","R"]
["C4.6",3036532,"T/Joints PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 75mm PVC.","Per item",25,"R","R"]
["C4.7",3036531,"T/Joints PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 63mm PVC.","Per item",25,"R","R"]
["C4.8",3036530,"T/Joints PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 50mm PVC.","Per item",25,"R","R"]
["C4.9",3036529,"T/Joints PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 25mm PVC.","Per item",30,"R","R"]
["C4.10",3035182,"T/Joints PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 20mm PVC.","Per item",30,"R","R"]
["C5",null,"FLANGES AND VALVES"]
["C5.1",3036542,"Stub flanges PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 250mm PVC.","Per item",15,"R","R"]
["C5.2",3036541,"Stub flanges PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 200mm PVC.","Per item",15,"R","R"]
["C5.3",3036540,"Stub flanges PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 160mm PVC.","Per item",15,"R","R"]
["C5.4",3036539,"Stub flanges PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 110mm PVC.","Per item",15,"R","R"]
["C5.5",3036538,"Stub flanges PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 90mm PVC.","Per item",15,"R","R"]
["C5.6",3035183,"Stub flanges PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 75mm PVC.","Per item",15,"R","R"]
["C5.7",3036551,"Butterfly valves with stainless steel disc, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 150mm 16 bar gear operated.","Per item",2,"R","R"]
["C5.8",3036555,"Butterfly valves with stainless steel disc, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 150mm PN16 lever operated.","Per item",2,"R","R"]
["C5.9",3036550,"Butterfly valves with stainless steel disc, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 250mm PVC Gear operated.","Per item",2,"R","R"]
["C5.10",3036554,"Butterfly valves with stainless steel disc, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 200mm PVC Lever Operated.","Per item",2,"R","R"]
["C5.11",3036549,"Butterfly valves with stainless steel disc, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 200mm PVC Gear Operated.","Per item",2,"R","R"]
["C5.12",3036553,"Butterfly valves with stainless steel disc, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 100mm PVC Lever operated.","Per item",2,"R","R"]
["C5.13",3036552,"Butterfly valves with stainless steel disc, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 80mm PVC Lever Operated.","Per item",2,"R","R"]
["C5.14",3036548,"Ball valves PVC, pressure nominal 16 bar @ 20°C water temp (PN16) single union","Supply and replace 110mm PVC.","Per item",15,"R","R"]
["C5.15",3036547,"Ball valves PVC, pressure nominal 16 bar @ 20°C water temp (PN16) Singel Union","Supply and replace 90mm PVC.","Per item",30,"R","R"]
["C5.16",3036546,"Ball valves PVC, pressure nominal 16 bar @ 20°C water temp (PN16) single union","Supply and replace 75mm PVC.","Per item",30,"R","R"]
["C5.17",3036545,"Ball valves PVC, pressure nominal 16 bar @ 20°C water temp (PN16) single union","Supply and replace 63mm PVC.","Per item",20,"R","R"]
["C5.18",3036544,"Ball valves PVC, pressure nominal 16 bar @ 20°C water temp (PN16) Singel union","Supply and replace 50mm PVC.","Per item",10,"R","R"]
["C5.19",3036543,"Ball valves PVC, pressure nominal 16 bar @ 20°C water temp (PN16) Singel union","Supply and replace 25mm PVC.","Per item",5,"R","R"]
["C6",null,"REDUCING BUSHES"]
["C6.1",3036378,"Reducing bushes PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 250/200mm.","Per item",15,"R","R"]
["C6.2",3036377,"Reducing bushes PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 200/160mm.","Per item",15,"R","R"]
["C6.3",3036376,"Reducing bushes PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 160/110mm.","Per item",15,"R","R"]
["C6.4",3036375,"Reducing bushes PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 110/90mm.","Per item",15,"R","R"]
["C6.5",3036374,"Reducing bushes PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 90/75mm.","Per item",15,"R","R"]
["C6.6",3036373,"Reducing bushes PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 75/63mm.","Per item",15,"R","R"]
["C6.7",3036372,"Reducing bushes PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 63/50mm.","Per item",15,"R","R"]
["C6.8",3036371,"Reducing bushes PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 50/25mm.","Per item",15,"R","R"]
["C6.9",3035184,"Reducing bushes PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 25/20mm.","Per item",15,"R","R"]
["C7",null,"SUPPORT CLIPS AND BACKING RINGS"]
["C7.1",3036386,"Support clips PVC","Supply and replace 200mm.","Per item",25,"R","R"]
["C7.2",3036385,"Support clips PVC","Supply and replace 160mm.","Per item",25,"R","R"]
["C7.3",3036384,"Support clips PVC","Supply and replace 110mm.","Per item",30,"R","R"]
["C7.4",3036383,"Support clips PVC","Supply and replace 90mm.","Per item",30,"R","R"]
["C7.5",3036382,"Support clips PVC","Supply and replace 75mm.","Per item",30,"R","R"]
["C7.6",3036381,"Support clips PVC","Supply and replace 63mm.","Per item",30,"R","R"]
["C7.7",3036380,"Support clips PVC","Supply and replace 50mm.","Per item",30,"R","R"]
["C7.8",3036379,"Support clips PVC","Supply and replace 25mm.","Per item",30,"R","R"]
["C7.9",3035185,"Support clips PVC","Supply and replace 20mm.","Per item",30,"R","R"]
["C7.10",3036390,"B/rings Galvanised","Supply and replace 160mm.","Per item",10,"R","R"]
["C7.11",3036389,"B/rings Galvanised","Supply and replace 110mm.","Per item",10,"R","R"]
["C7.12",3036388,"B/rings Galvanised","Supply and replace 90mm.","Per item",10,"R","R"]
["C7.13",3036387,"B/rings Galvanised","Supply and replace 75mm.","Per item",10,"R","R"]
["C8",null,"BOLTS AND NUTS"]
["C8.1",3036563,"Bolts & nuts & washers (m16) zinc platted","Supply and replace 250mm long.","Per item",100,"R","R"]
["C8.2",3036562,"Bolts & nuts & washers (m16) zinc platted","Supply and replace 200mm long.","Per item",100,"R","R"]
["C8.3",3036561,"Bolts & nuts & washers (m16) zinc platted","Supply and replace 160mm long.","Per item",100,"R","R"]
["C8.4",3036560,"Bolts & nuts & washers (m16) zinc platted","Supply and replace 125mm long.","Per item",100,"R","R"]
["C8.5",3036559,"Bolts & nuts & washers (m16) zinc platted","Supply and replace 110mm.","Per item",100,"R","R"]
["C8.6",3036558,"Bolts & nuts & washers (m16) zinc platted","Supply and replace 100mm long.","Per item",100,"R","R"]
["C8.7",3036557,"Bolts & nuts & washers (m16) zinc platted","Supply and replace 75mm long.","Per item",100,"R","R"]
["C8.8",3036556,"Bolts & nuts & washers (m16) zinc platted","Supply and replace 63mm long.","Per item",100,"R","R"]
["C9",null,"UNIONS"]
["C9.1",3036571,"Unions PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 110mm.","Per item",10,"R","R"]
["C9.2",3036570,"Unions PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 90mm.","Per item",10,"R","R"]
["C9.3",3036569,"Unions PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 75mm.","Per item",10,"R","R"]
["C9.4",3036568,"Unions PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 63mm.","Per item",10,"R","R"]
["C9.5",3036567,"Unions PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 50mm.","Per item",10,"R","R"]
["C9.6",3036566,"Unions PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 25mm.","Per item",10,"R","R"]
["C9.7",3036565,"Unions PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 20mm.","Per item",10,"R","R"]
["C9.8",3036564,"Aim-flow PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 50mm.","Per item",10,"R","R"]
["C10",null,"VALVES"]
["C10.1",3036572,"Non return valves PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace 50mm.","Per item",15,"R","R"]
["C10.2",3035188,"Non return valves PVC, pressure nominal 16 bar @ 20°C water temp (PN16)","Supply and replace25mm.","Per item",15,"R","R"]
["C11",null,"CONSUMABLES"]
["C11.1",3036856,"PVC glue","Supply and apply 500ml PVC cement (16 Bar pressure).","500ml",150,"R","R"]
["C11.2",3036857,"PVC Etch cleaner","Supply and apply 500ml PVC Etch.","500ml",150,"R","R"]
["C12",null,"PRESSURE TESTING"]
["C12.1",3035189,"Up to 63mm pipes","Do a complete pressure test on circuits up to 50 meters length of pipe.","Per 50 meter",10,"R","R"]
["C12.2",3035190,"Between 63mm up to 250mm","Do a complete pressure test on circuits up to 50 meters length of pipe.","Per 50 meter",5,"R","R"]
["Total for Category C (Excluding VAT)",{"$nulls":6},"R"]
[]
["D",null,"INDUSTRIAL FILTERS, WEIRS AND LEAF CATCHERS ETC"]
["D1",null,"STRAINERS"]
["D1.1",3035191,"Strainer in line","Supply and replace 25mm plastic discs on chlorine injector line.","Per item",25,"R","R"]
["D1.2",3035193,"Plastic filter - 3 bag","Supply and replace plastic filter 3 bag, new complete with multiport valve.","Per item",10,"R","R"]
["D1.3",3035194,"Plastic filter - 4 bag","Supply and replace plastic filter 4 bag new complete with multiport valve.","Per item",10,"R","R"]
["D1.4",3036391,"Plastic filter - 5 bag","Supply and replace plastic filter 5 bag, new complete with multiport valve.","Per item",10,"R","R"]
["D1.5",3036392,"Plastic filter modules - 3 bag, service parts","Supply and replace filter media underdrains, turrets, elements, filter lid, seal, stainless steel screws, tank connector with O-piping internal, air releases.","Per item",15,"R","R"]
["D1.6",3035192,"Plastic filter modules - 4 bag, service parts","Supply and replace filter media underdrains, turrets, elements, filter lid, seal, stainless steel screws, tank connector with O-piping internal, air releases.","Per item",15,"R","R"]
["D1.7",3036393,"Plastic filter modules - 5 bag, service parts","Supply and replace filter media underdrains, turrets, elements, filter lid, seal, stainless steel screws, tank connector with O-piping internal, air releases.","Per item",15,"R","R"]
["D1.8",3036394,"Fibreglass filter - 8 bag","Supply and replace fibreglass filter 8 bag, inlet and outlet 2 inch new complete. Filter connectors must be SABS approved (SANS 1808-5).","Per item",15,"R","R"]
["D1.9",3036395,"Fibreglass filter - 12 bag","Supply and replace fibreglass filter 12 bag, inlet and outlet 2 inch new complete. Filter connectors must be SABS approved (SANS 1808-5).","Per item",10,"R","R"]
["D1.10",3036396,"Fibreglass re-enforced filter modules 6 bag- service parts","Supply and replace filter media, 1 x Hydro-Anthracite, 6 bag media underdrains, 250mm & 350mm elements filter lids, seals, turrets, piping & internal air releases.","Per item",20,"R","R"]
["D1.11",3036397,"Fibreglass re-enforced filter modules 12 bag - service parts","Supply and replace filter media, 2 x Hydro-Anthracite, 12 bag media underdrains, 250mm & 350mm elements filter lids, seals, turrets, piping & internal air releases.","Per item",20,"R","R"]
["D1.12",3035195,"Leaf catcher MK 1 - complete re-enforced","Supply and replace 20L Stainless steel baskets with 5mm holes.","Per item",10,"R","R"]
["D1.13",3035196,"Leaf catcher MK 1 - complete re-enforced","Supply and replace 20L Fiberglass leaf catcher new complete housing, lid, bolts and nuts.","Per item",10,"R","R"]
["D1.14",3035198,"Leaf catcher MK 2 - complete re-enforced","Supply and replace 40L Stainless steel baskets with 5mm holes.","Per item",10,"R","R"]
["D1.15",3035197,"Leaf catcher MK 2 - complete re-enforced","Supply and replace 40L Fiberglass leaf catcher new complete housing, lid, bolts and basket.","Per item",10,"R","R"]
["D1.16",3035199,"Leaf Catcher MK1","Supply and replace only lid, bolts and O ring.","Per item",10,"R","R"]
["D1.17",3035200,"Leaf Catcher MK2","Supply and replace only lid, bolts and O ring.","Per item",10,"R","R"]
["D1.18",3035201,"Industrial multi-port valve 2 inch on filter system. Flow rate not smaller than 14 m³, Large Body Imported","Supply and replace industrial multi-port valve .","Per item",10,"R","R"]
["D1.19",3035202,"Multi-port valve 1,5 inch. Flow rate not smaller than 9,7 m³","Supply and replace industrial multi-port valve.","Per item",15,"R","R"]
["D2",null,"FILTERS, WEIRS AND LEAF CATCHERS"]
["D2.1",200000045102,"Weirs - Industrial","Supply only deck lids Ø450mm reinforced fibreglass.","Per item",25,"R","R"]
["D2.2",3035204,"Weirs - Industrial","Supply and replace deck lids Ø450mm reinforced fibreglass.","Per item",25,"R","R"]
["D2.3",3000770,"Weirs - Industrial","Supply and replace industrial weirs fibreglass new complete with deck lid, basket, vacuum lid and body.","Per item",5,"R","R"]
["D2.4",200000045105,"Weirs - Industrial","Supply only fibreglass vacuum lids Ø450mm.","Per item",10,"R","R"]
["D2.5",3000826,"Weirs - Industrial","Supply and replace fibreglass vacuum lids Ø450mm.","Per item",10,"R","R"]
["D2.6",200000045106,"Weirs - Industrial","Supply only baskets Ø400mm Stainless steel mesh reinforced.","Per item",10,"R","R"]
["D2.7",3026858,"Weirs - Industrial","Supply and replace baskets Ø400mm Stainless steel mesh reinforced.","Per item",10,"R","R"]
["D2.8",3026306,"Weirs – Domestic","Supply and replace new complete weir including Vacuum lid, deck lid, basket and body.","Per item",10,"R","R"]
["D2.9",200000045108,"Weirs - Domestic","Supply only plastic deck lids Ø250mm.","Per item",20,"R","R"]
["D2.10",3026311,"Weirs - Domestic","Supply and replace plastic deck lids Ø250mm.","Per item",20,"R","R"]
["D2.11",200000045109,"Weirs - Domestic","Supply only vacuum lids Ø250mm.","Per item",20,"R","R"]
["D2.12",3027998,"Weirs - Domestic","Supply and replace vacuum lids Ø250mm.","Per item",20,"R","R"]
["D2.13",200000045763,"Weirs - Domestic","Supply only baskets Ø200mm.","Per item",20,"R","R"]
["D2.14",3029180,"Weirs - Domestic","Supply and replace baskets Ø200mm.","Per item",20,"R","R"]
["Total for Category D (Excluding VAT)",{"$nulls":6},"R"]
[]
["E1",null,"CHLORINE GAS EQUIPMENT"]
["E1.1",200000045789,"Complete compact dosing regulator VGB-103","Supply only new complete regulator 0-250g/hr.","Per item",10,"R","R"]
["E1.2",3035206,"Complete compact dosing regulator VGB-103","Service complete regulator 0-250g/hr.","Per item",10,"R","R"]
["E1.3",200000045791,"Complete compact dosing regulator VGB-103","Supply only new complete regulator 0-500g/hr.","Per item",10,"R","R"]
["E1.4",3036573,"Complete compact dosing regulator VGB-103","Service complete regulator 0-500g/hr.","Per item",10,"R","R"]
["E1.5",200000045822,"Complete compact dosing regulator VGB-103","Supply only new complete regulator 0-1000g/hr.","Per item",10,"R","R"]
["E1.6",3036574,"Complete compact dosing regulator VGB-103","Service complete regulator 0-1000g/hr.","Per item",10,"R","R"]
["E1.7",3036575,"Service kit spares VGB-103 casing / housing","Supply and replace Casing/housing.","Per item",15,"R","R"]
["E1.8",3036576,"Service kit spares VGB-103 ","Supply and replace O-rings.","Per item",15,"R","R"]
["E1.9",3036577,"Service kit spares VGB-103","Supply and replace diaphragm.","Per item",15,"R","R"]
["E1.10",3036578,"Service kit spares VGB-103","Supply and replace filters & gaskets.","Per item",15,"R","R"]
["E1.11",3036579,"Service kit spares VGB-103","Supply and replace flow glass with seals 0-250g/hr.","Per item",15,"R","R"]
["E1.12",3036580,"Service kit spares VGB-103","Supply and replace flow glass with seals 0-500g/hr.","Per item",15,"R","R"]
["E1.13",3036581,"Service kit spares VGB-103","Supply and replace flow glass with seals 0-1000g/hr.","Per item",15,"R","R"]
["E1.14",3036582,"Service kit spares VGB-103","Supply and replace flow spindle (rate valve) 0-500g/hr.","Per item",15,"R","R"]
["E1.15",3036583,"Service kit spares VGB-103","Supply and replace flow spindle (rate valve) 0-1000g/hr.","Per item",15,"R","R"]
["E1.16",3036584,"Service kit spares VGB-103","Supply and replace Intake valve.","Per item",15,"R","R"]
["E1.17",3036585,"Service kit spares VGB-103","Supply and replace Yoke assembly.","Per item",15,"R","R"]
["E1.18",3036586,"Service kit spares VGB-103","Supply and replace Gas vacuum line 25m.","25 meter",15,"R","R"]
["E1.19",3036587,"new complete PVC injector for Chlorine gas","Supply and replace 0.5 4.0 KG/HR with non-return diaphragm.","Per item",15,"R","R"]
["E1.20",3036588,"Service kit for Chlorine gas injector","Supply and replace O-diaphragm, Teflon seals, spring and seals.","Per item",15,"R","R"]
["E1.21",200000045124,"Cylinder Chlorine Gas Spanner","Supply only Spanner to open and close cylinder.","Per item",25,"R","R"]
["E1.22",3036589,"Chlorine gas detector","Supply and replace new complete gas detector controller & sensor: Refer to 3.1 Specification details.","Per item",1,"R","R"]
["E1.23",3036590,"Chlorine gas detector","Supply and replace new complete gas leak detector sensor.","Per item",2,"R","R"]
["E1.24",3035208,"Kit A Chlorine emergency repair kit in a durable Yellow polyethylene or steel trunk kit box with 2 x pad locks (one key opens both locks) including installation of an emergency key box","Supply only a Chlorine emergency repair kit. Refer to 3.1 Specification details for the detailed list of items required for the chlorine emergency repair kit.","Per item",5,"R","R"]
["E1.25",200000045126,"Full face mask activated gasp Protection chin-type gas mask","Supply only chlorine full face gas mask twin canister.","Per item",30,"R","R"]
["E1.26",200000045127,"B2P3 Canisters","Supply only B2P3 for full face gas mask twin canister.","Per item",15,"R","R"]
["E1.27",200000045823,"3S Basic Plus Full Face Mask","Supply only chlorine full face gas mask single canister.","Per item",10,"R","R"]
["E1.28",200000045824,"Single Mask HAZMAT canister","Supply only a single Hazardous Materials (HAZMAT) canister for full face gas mask.","Per item",10,"R","R"]
["E1.29",200000045128,"2pc Chemical resistant and waterproof PVC full arm gloves","Supply only chemical resistant and waterproof Full Arm up to shoulder.","Per set",30,"R","R"]
["E1.30",200000045154,"Platform scale for single Gas Cylinder weight","Supply and replace with new complete platform scale. Refer to 3.1 Specification details","Per item",10,"R","R"]
["E1.31",200000045825,"Platform scale for double Gas Cylinder weight","Supply and replace with new complete platform scale. Refer to 3.1 Specification details","Per item",10,"R","R"]
["E1.32",3036591,"Platform scale calibration certificate","Supply calibration certificate.","Per item",20,"R","R"]
["E1.33",200000045826,"Single Cylinder Trolley with chain.","Supply single cylinder trolley that is fitted with rubber wheels and a galvanised chain to hold cylinders securely. Size - 1050mm H x 483mm  W 520mm x D. Trolley capacity 150kgs. Maximum cylinder allowance Ø280mm. Wheels minimum Ø200mm).","Per item",30,"R","R"]
["E1.34",3036592,"Signage \"No Match\" (open flames) PV 2","Supply and replace red on white 290mm x 290mm standard on PVC backing and mounted to the wall with screws. Signage must comply with SANS 10134:2016.","Per item",30,"R","R","sans 1419"]
["E1.35",3036593,"Signage \"No Match\" (open flames) PV 3","Supply and replace red on white 440mm x 440mm standard on PVC backing and mounted to the wall with screws. Signage must comply with SANS 10134:2016.","Per item",30,"R","R"]
["E1.36",3036594,"Signage \"No Smoking\" PV 1","Supply and replace red on white 290mm x 290mm standard on PVC backing and mounted to the wall with screws. Signage must comply with SANS 10134:2016.","Per item",30,"R","R"]
["E1.37",3036595,"Signage \"No Smoking\" PV 2","Supply and replace red on white 440mm x 440mm standard on PVC backing and mounted to the wall with screws. Signage must comply with SANS 10134:2016.","Per item",30,"R","R"]
["E1.38",3036596,"Signage \"No Entry\" PV 6","Supply and replace red on white 290mm x 290mm standard on PVC backing and mounted to the wall with screws. Signage must comply with SANS 10134:2016.","Per item",30,"R","R"]
["E1.39",3036597,"Signage \"No Entry\" PV 6","Supply and replace red on white 440mm x 440mm standard on PVC backing and mounted to the wall with screws. Signage must comply with SANS 10134:2016.","Per item",30,"R","R"]
["E1.40",3036598,"Signage \"Wear gloves” MV 5","Supply and replace blue on white 290mm x 290mm standard on PVC backing and mounted to the wall with screws. Signage must comply with SANS 10134:2016.","Per item",30,"R","R"]
["E1.41",3036599,"Signage \"Wear gloves” MV 5","Supply and replace blue on white 440mm x 440mm standard on PVC backing and mounted to the wall with screws. Signage must comply with SANS 10134:2016.","Per item",30,"R","R"]
["E1.42",3036600,"Signage \"Wear overall\" MV 20","Supply and replace blue on white 290mm x 290mm standard on PVC backing and mounted to the wall with screws. Signage must comply with SANS 10134:2016.","Per item",30,"R","R"]
["E1.43",3036601,"Signage \"Wear overall\" MV 20","Supply and replace blue on white 440mm x 440mm standard on PVC backing and mounted to the wall with screws. Signage must comply with SANS 10134:2016.","Per item",30,"R","R"]
["E1.44",3036602,"Signage \"Wear safety shoes\" MV 7","Supply and replace blue on white 290mm x 290mm standard on PVC backing and mounted to the wall with screws. Signage must comply with SANS 10134:2016.","Per item",30,"R","R"]
["E1.45",3036603,"Signage \"Wear safety shoes\" MV 7","Supply and replace blue on white 440mm x 440mm standard on PVC backing and mounted to the wall with screws. Signage must comply with SANS 10134:2016.","Per item",30,"R","R"]
["E1.46",3036604,"Signage \"Wear Apron” MV 9","Supply and replace blue on white 290mm x 290mm standard on PVC backing and mounted to the wall with screws. Signage must comply with SANS 10134:2016.","Per item",30,"R","R"]
["E1.47",3036605,"Signage \"Wear Apron” MV 9","Supply and replace blue on white 440mm x 440mm standard on PVC backing and mounted to the wall with screws. Signage must comply with SANS 10134:2016.","Per item",30,"R","R"]
["E1.48",3036606,"Signage \"Warning of Poisons Substance Hazard” WW 5 ","Supply and replace blue on white 290mm x 290mm standard on PVC backing and mounted to the wall with screws. Signage must comply with SANS 10134:2016.","Per item",30,"R","R"]
["E1.49",3036607,"Signage \"Warning of Poisons Substance Hazard” WW 5 ","Supply and replace blue on white 440mm x 440mm standard on PVC backing and mounted to the wall with screws. Signage must comply with SANS 10134:2016.","Per item",30,"R","R"]
["E1.50",3036608,"Signage \"Wear Chlorine Mask” MV 2","Supply and replace blue on white 290mm x 290mm standard on PVC backing and mounted to the wall with screws. Signage must comply with SANS 10134:2016.","Per item",30,"R","R"]
["E1.51",3036609,"Signage \"Wear Chlorine Mask” MV 2","Supply and replace blue on white 440mm x 440mm standard on PVC backing and mounted to the wall with screws. Signage must comply with SANS 10134:2016.","Per item",30,"R","R"]
["E1.52",3036610,"Signage \"Fire extinguisher\" FB 2","Supply and replace red on white 290mm x 290mm standard on PVC backing and mounted to the wall with screws. Signage must comply with SANS 10134:2016.","Per item",30,"R","R"]
["E1.53",3036611,"Signage \"Fire extinguisher\" FB 2","Supply and replace red on white 440mm x 440mm standard on PVC backing and mounted to the wall with screws. Signage must comply with SANS 10134:2016.","Per item",30,"R","R"]
["E1.54",3036612,"Signage \"Red Arrow\" FB 1","Supply and replace red on white 290mm x 290mm standard on PVC backing and mounted to the wall with screws. Signage must comply with SANS 10134:2016.","Per item",30,"R","R"]
["E1.55",3036613,"Signage \"Red Arrow\" FB 1","Supply and replace red on white 440mm x 440mm standard on PVC backing and mounted to the wall with screws. Signage must comply with SANS 10134:2016.","Per item",30,"R","R"]
["Total for Category E (Excluding VAT)",{"$nulls":6},"R"]
[]
["F1",null,"EARTHWORKS"]
["F1.1",3035209,"Remove existing paving","Remove existing paving and prepare surface with plate compacting to replace existing paving.","m2",100,"R","R"]
["F1.2",3035210,"Demolish existing concrete structures","Demolish with Pneumatic tools or hand and rubble removal as per F9.1.","m3",10,"R","R"]
["F1.3",3035211,"Demolish brick walls","Demolish with Pneumatic tools or hand and rubble removal as per F9.1.","m2",10,"R","R"]
["F1.4",3035212,"Concrete coring and drilling","Supply and service - drilling Up to 50mm.","Per Hole",10,"R","R"]
["F1.5",3035213,"Concrete coring and drilling","Supply and service - drilling Up to 50/100mm.","Per Hole",10,"R","R"]
["F2",null,"EXCAVATION, FILLING, ETC."]
["F2.1",3035214,"Excavation in earth not exceeding 1m deep","Excavate intermediate Material - Hand or machine excavation. Material that requires back-acting excavator of flywheel power exceeding 0,10 kw per millimeter of tined-bucket width or the use of pneumatic tools.","m3",150,"R","R"]
["F2.2",3035215,"New Trenching","Supply and service - Trenching 1m x 500mm x 500mm by hand or pneumatic tools.","Per meter",150,"R","R"]
["F2.3",3035216,"Stabilizing of backfill material.","Supply and service - Stabilize with 5% cement /m3 to Optimum moisture content (OMC).","m3",150,"R","R"]
["F2.4",3035217,"Backfilling and compaction of trenches, holes etc.","Supply and service - compaction to 95% Mod AASTHO. ","m3",150,"R","R"]
["F2.5",3035218,"Compaction of surfaces","Supply and service - compaction of surfaces under paving etc. with a plate compactor to 95% Mod AASTHO.","m2",150,"R","R"]
["F3",null,"CONCRETE, FORMWORK AND REINFORCEMENT"]
["F3.1",3035219,"25MPa/19mm concrete","Supply and replace concrete with a minimum compressive strength of 25Mpa after 28 days.","m3",100,"R","R"]
["F3.2",3035220,"Reinforced concrete","Supply and replace 30mpa reinforced 150/200mm thick concrete with ref.100 mesh (200mm x 200m x 4mm wire) with Y10 reinforced rods, 500mm x 500mm apart.","m2",100,"R","R"]
["F3.3",3035221,"Screed Plaster","Supply and service - Plaster a thin, top layer (20mm) of material (sharp sand and cement, similarly to concrete) over a concrete subfloor on concrete. Cement to sand ratio Minimum 1:3 or 1:4 and compressive strength 20 MPa.","m2",100,"R","R"]
["F3.4",3035222,"Cement Plaster","Supply and service - apply cement plaster screeds steel trowelled, using the delayed trowelling method on concrete 70mm. Plaster shall be CEM I strength class 32.5N complying with SANS 50197/1 or masonry cement strength class 22.5 X complying with SANS 50413/1.","m2",100,"R","R"]
["F3.5",3035223,"Concrete finishing","Supply and service - finishing top surfaces of concrete smooth with a steel float.","m2",100,"R","R"]
["F3.6",3035224,"Waterproofing","Supply and service - apply one layer 250-micron polyethylene waterproof sheeting under surface beds.","m2",100,"R","R"]
["F4",null,"Pool Outdoor Furniture "]
["F4.1",3036614,"Exposed Aggregate Braai","Supply and replace - Braai stand with overall hight 950mm, height above ground: 900mm diameter: 500mm and finish in exposed aggregate.","Pre Item",30,"R","R"]
["F4.2",3036615,"Exposed Aggregate Drinking fountain","Supply and replace - drinking fountain with height overall 1200mm, height above ground 900mm, diameter 300mmand finish in exposed aggregate.","Pre Item",30,"R","R"]
["F4.3",3036616,"Concrete Bollards Park","Supply and replace - Bollards with height 1400 mm, diameter 330 mm and Base Diameter 330 mm, weight 291 kg.","Pre Item",100,"R","R"]
["F4.4",3036617,"Concrete Bollards Major","Supply and replace - Bollards with height 760 mm, diameter 150 mm and Base Diameter 200 mm, weight 45 kg.","Pre Item",100,"R","R"]
["F4.5",3036618,"Seat precast concrete block seat","Supply and replace - seat with length 500mm, height 410 mm, width 500 mm.","Pre Item",30,"R","R"]
["F4.6",3036619,"Bench precast concrete bench","Supply and replace - Size: 1600mm long x 500mm wide x 500mm high, Mass: 305kg, with finish in smooth natural grey concrete. Top edge chamfered all around. Concrete 30MPa steel reinforced.","Pre Item",30,"R","R"]
["F4.7",200000045827,"Recycled Plastic Picnic set","Supply and replace - 6-Seater and Table made from 100% recycled plastic 1580mm 1510mm.","Pre Item",30,"R","R"]
["F5",null,"REINFORCEMENT"]
["F5.1",200000045129,"Concrete reinforcing","Supply and service - Type 193 fabric reinforcement in concrete surface beds, slabs, etc 2400mm x 600mm x 5.6, weight 28kg reinforcement mesh.","Per sheet",100,"R","R"]
["F5.2",200000045130,"Concrete reinforcing","Supply and service - Mild steel reinforcement Y10 (10mm round steel bar) in structural concrete.","Kg",100,"R","R"]
["F6",null,"BRICK WORK FOR RETAINING WALLS ETC"]
["F6.1",3035225,"Brick work","Supply and service - 115mm brick walls with NFX bricks with a minimum compressive strength of 7Mpa. Cement Mortar consist of 1 part of common cement (CEM I) to 6 parts of sand volume for mortar class II.","m2",100,"R","R"]
["F6.2",3035226,"Brick work","Supply and service - 230mm brick walls with NFX bricks with a minimum compressive strength of 7Mpa. Cement Mortar consist of 1 part of common cement (CEM I) to 6 parts of sand volume for mortar class II.","m2",100,"R","R"]
["F6.3",3036620,"Face brick","Supply and service - Extra over for FBX semi-face brick with a minimum compressive strength of 14Mph. Brick strength must comply with SANS 227 specifications.","m2",100,"R","R"]
["F6.4",3035227,"Cement Plaster","Supply and service - Two coat plaster average 25mm thick on brick walls. Plaster shall be CEM I strength class 32.5N complying with SANS 50197/1 or masonry cement strength class 22.5 X complying with SANS 50413/1.","m2",100,"R","R"]
["F7",null,"PAINTING"]
["F7.1",3035228,"Acrylic low sheen paint on internal plastered walls","Supply and service - Prepare, stop and apply one coat plaster primer on surface, one Universal undercoat and two coats Low sheen\" acrylic paint in accordance with SANS 1586.","m2",100,"R","R"]
["F7.2",3035229,"Paint on external plastered walls","Supply and service - apply one coat bonding liquid and two coats exterior quality PVC emulsion paint in accordance with SANS 1586.","m2",100,"R","R"]
["F7.3",3035230,"Paint on rails, bars, pipes, etc not exceeding 150mm diameter","Supply and service - Remove all loose or flaking paint and rust and apply one coat zinc chromate primer, one coat universal undercoat and two coats enamel paint.","Per meter",100,"R","R"]
["F7.4",3035231,"Timber Preservative Coating - (odourless, waxed-based, water-repelling coating.)","Supply and service - apply waxed-based timber preservative coating on timber structures bollards and railings etc.","Per meter",100,"R","R"]
["F7.5",3035232,"Creosote","Supply and service - apply creosote on timber structures, bollards and railings etc.","Per meter",100,"R","R"]
["F8",null,"PAVING"]
["F8.1",3036621,"100GSM Poly woven fabric weed barrier material","Supply and replace weed barrier material under paving area.","m2",100,"R","R"]
["F8.2",3036622,"Herbicide treatment","Supply and service - treat area under paving area with herbicides.","m2",100,"R","R"]
["F8.3",3035233,"Coarse river sand filling","Supply and replace - Sand blinding to trenches or under paving average 25mm thick.","m2",500,"R","R"]
["F8.4",3035234,"Paving Interlock pavers","Supply and replace with new interlock pavers 200 x 98.5 x 70mm. Average Comp Strength 47.0.","m2",500,"R","R"]
["F8.5",3036623,"Paving Interlock pavers - lift and replace","Repair and replace existing interlock pavers 200 x 98.5 x 70mm. Average Comp Strength 47.0.","m2",250,"R","R"]
["F8.6",3036624,"Polymeric sand sealer","Supply and replace polymeric sand between pavers to seal the Interlock pavers 200 x 98.5 x 70mm. Average Comp Strength 47.0.","m2",100,"R","R"]
["F8.7",3035235,"Bull nose copings Clay/Cement pavers","Supply and replace damaged Bull nose copings Clay/Cement pavers with new.","Per meter",250,"R","R"]
["F8.8",3035236,"Storm Water Channel, drainage around pools","Supply and replace sections of the plastic channel with grid and connector. Wide 110mm depth 75mm.","Per meter",500,"R","R"]
["F8.9",3036859,"Storm Water Channel, drainage around pools","Supply and replace sections of the concrete channel with grid and pipe drain connector. Wide 110mm depth 75mm.","Per meter",500,"R","R"]
["F9",null,"SITE CLEANING"]
["F9.1",3035237,"Rubble removal","Supply and service - The Contractor shall clean the work area and remove all rubble to an approved dumping site.","m3",150,"R","R"]
["Total for Category F (Excluding VAT)",{"$nulls":6},"R"]
[]
["G1",null,"TILING AND FIBREGLASS"]
["G1.1",3035238,"Removal of existing tiles","Supply and service - Chopping off existing tiles and preparing surface to take new tiles.","m2",200,"R","R"]
["G1.2",3035239,"Inner surface","Supply and repair - Prepare and clean the surface: remove any debris, loose tiles, and old adhesive. Repair any cracks or damage, and ensure the surface is smooth and level before applying a waterproofing membrane to prevent future issues. Finally, allow the surface to dry completely before applying the new tile adhesive. ","m2",500,"R","R"]
["G1.3",3035240,"Inner surface cleaning","Supply and service - Prepare and clean with Hydrochloric acid when removing stains.","m2",250,"R","R"]
["G1.4",3035241,"Emptying of Pool","Supply and service - Per 10 000ℓ & cleaning pool inner surface.","Per 10 000ℓ ",125,"R","R"]
["G1.5",3036627,"Tiles","Supply and replace mosaics 50mm x 50mm tiles. 150 wide, Ceramic Cobalt Blue & Black.","Per running meter",200,"R","R"]
["G1.6",3036628,"Tiles","Supply and replace mosaics 300mm x 300mm tiles sheet. Cobalt Blue & Black.","Per meter",200,"R","R"]
["G1.7",3036625,"Tiles","Supply and replace Johnson White 150mm x 150mm Ceramic tiles.","m2",200,"R","R"]
["G1.8",3036860,"Tiles","Supply and replace Johnson White 152mm x 152mm Ceramic.","m2",200,"R","R"]
["G1.9",3036626,"Tiles","Supply and replace Shiny White 200mm x 200mm.","m2",200,"R","R"]
["G1.10",3036629,"Marbelite ","Supply, repair and prepare surface for application.","m2",1000,"R","R"]
["G1.11",3035243,"Outside around pool expansion joint","Supply, repair and prepare surface for application 50mm x 10mm (surface high density foam).","Per running meter",200,"R","R"]
["G1.12",3035244,"Underwater expansion joint","Supply, repair and prepare surface for application submerged and filler material 15mm x 15mm.","Per running meter",1000,"R","R"]
["G1.13",3035245,"Underwater expansion joint","Service - removal of old expansion joint material.","Per running meter",1000,"R","R"]
["G1.14",3036630,"Waterproof tile grout inner surface tile floor.","Supply, repair and prepare surface for application of grouting up to 20mm x 8mm with bonding liquid.","m2",4000,"R","R"]
["G1.15",3035246,"Submerge underwater and replace loose tiles with watertight grout and adhesive for inner surface tile floor. ","Prepare and replace broken and loose tiles by submerging underwater with watertight grout and adhesive for inner surface tile floor. ","m2",1000,"R","R"]
["G1.16",3035242,"Repair mortar with integral corrosion inhibitors","Supply and apply a quick-setting, low shrinkage repair mortar to seal water collection areas. The product must comply with NSF/ANSI standard 61.","25kg",200,"R","R"]
["G2",null,"FIBREGLASS"]
["G2.1",3035247,"Fibreglass (Chopped Strand Mat)","Supply and replace with new 450g/ m² at prime resin & pool cote and finishing surface.","m2",500,"R","R"]
["G2.2",3035248,"Fibreglass repair","Supply, repair and prepare pool for coat with at prime 7 final coat.","m2",2000,"R","R"]
["G2.3",3036631,"Printed Fibreglass mosaic tile sheet","Supply and replace printed Fibreglass mosaic tile sheet 300mm x 300mm.","Per running meter",500,"R","R"]
["G2.4",3035249,"Dry Fix Epoxy Pond, Swimming Pool & Floor Coating Two Part Paint Kit (5L) Cover 40m/2","Supply, apply and repair with a high build Epoxy Dawn Blue Part A (5L) and high build Epoxy Part B (5L).","Per Kit",100,"R","R"]
["G3",null,"SLIDES & TUBES"]
["G3.1",3035250,"Slides and tubes fiberglass","Supply and replace straight sections 2m length 1,250m wide.","Per item",10,"R","R"]
["G3.2",3035251,"Slides and tubes fiberglass","Supply and replace curved sections.","Per item",10,"R","R"]
["G3.3",3035252,"Slides and tubes fiberglass","Supply and replace stainless steel bolts & nuts 10mm.","Per item",100,"R","R"]
["G3.4",3035253,"Slides and tubes fiberglass","Supply, replace and repair section joints.","Per item",25,"R","R"]
["G3.5",3035254,"Slides and tubes fiberglass","Supply, replace and repair starting box, reinforcing and grid.","Per item",25,"R","R"]
["G3.6",3035255,"Slides and tubes fiberglass","Supply, replace and repair Chromated Copper Arsenate treated 110mm support poles in concrete.","Per item",25,"R","R"]
["G3.7",3035256,"Slides and tubes fiberglass","Supply and replace anchor bolts mounting.","Per item",25,"R","R"]
["G3.8",3035257,"Slides and tubes fiberglass","Supply and service - Treat wood with Chromated Copper Arsenate for durability support poles 110mm x 1m.","Per meter",25,"R","R"]
["G3.9",3035258,"Slides and tubes fiberglass","Supply and service - Paint top platform, rails, stairs and structures with waxed-based timber preservative coating (See Item F7.4).","m2",25,"R","R"]
["G3.10",3035259,"Slides and tubes","Supply, replace and repair decking pine fine ribbed H3 22mm x 102mm Chromated Copper Arsenate treated.","m2 ",25,"R","R"]
["Total for Category G (Excluding VAT)",{"$nulls":6},"R"]
[]
["H",null,"SWIMMING POOL ACCESSORIES"]
["H1",null,"STAINLESS STEEL GRAB RAILS"]
["H1.1",3036634,"Grab rails, 316 Stainless steel","Supply and replace Ø50mm Rails.","Per meter",20,"R","R"]
["H1.2",3036633,"Grab rails, 316 Stainless steel","Supply and replace Ø38mm Rails.","Per meter",20,"R","R"]
["H1.3",3036632,"Grab rails, 316 Stainless steel","Supply and replace Ø16mm Rails.","Per meter",20,"R","R"]
["H1.4",3035260,"Grab rails, 316 Stainless steel welding","Supply and repair - Welding rails per joint Ø 50/38/16mm.","Per item",40,"R","R"]
["H1.5",3035261,"Grab rails, 316 Stainless steel ","Supply and replace Grab rails 1,5mm wall thickness Ø 38 p/rail new complete with core drill and epoxy.","Per item",20,"R","R"]
["H1.6",3036635,"Grab rails, 316 Stainless steel","Supply and replace 316 Stainless steel bolts and nuts, chemical anchors with nozzle.","Per item",100,"R","R"]
["H1.7",3036636,"Drain lids, 316 Stainless steel","Supply and replace Stainless perforated lids 300 x 300mm floor drains - screws x 4 included.","Per item",100,"R","R"]
["H1.8",3035262,"Grids, 316 Stainless steel","Supply and service - Welding stainless Steel grids per 100mm.","Per item",100,"R","R"]
["H1.9",3036637,"Grid Moulded fiberglass grating made with isophthalic resin","Supply and replace - 25mm thick 38x38mm apertures.","Per item",100,"R","R"]
["H2",null,"SWIMMING LANES"]
["H2.1",200000045144,"Swimming lanes anti-turbulent discs","Supply only anti-turbulent discs Ø100mm.","Per item",200,"R","R"]
["H2.2",3036638,"Swimming lanes anti-turbulent discs","Supply and replace anti-turbulent discs Ø100mm.","Per item",200,"R","R"]
["H2.3",200000045145,"Swimming lanes anti-turbulent discs","Supply only anti-turbulent discs Ø150mm.","Per item",200,"R","R"]
["H2.4",3036639,"Swimming lanes anti-turbulent discs","Supply and replace anti-turbulent discs Ø150mm.","Per item",200,"R","R"]
["H2.5",200000045146,"Swimming lanes rope floats","Supply only rope floats. High density polyethylene Ø100mm.","Per item",200,"R","R"]
["H2.6",3036640,"Swimming lanes rope floats","Supply and replace rope floats. High density polyethylene Ø100mm.","Per item",200,"R","R"]
["H2.7",200000045147,"Swimming lanes rope floats","Supply only rope floats. High density polyethylene Ø150mm.","Per item",200,"R","R"]
["H2.8",3036641,"Swimming lanes rope floats","Supply and replace rope floats. High density polyethylene Ø150mm.","Per item",200,"R","R"]
["H2.9",3035263,"Stainless steel wire with hook attached one end","Supply and replace stainless steel wire 4mm x 50m long.","Per item",60,"R","R"]
["H2.10",200000045148,"Stainless steel ratchets for tensioning lanes spanner operated","Supply and replace stainless steel ratchet.","Per item",30,"R","R"]
["H2.11",3036642,"Turnbuckle, hook & eye","Supply and replace 6mm stainless steel turnbuckle.","Per item",30,"R","R"]
["H2.12",3036643,"Turnbuckle, hook & eye","Supply and replace 8mm stainless steel turnbuckle.","Per item",30,"R","R"]
["H2.13",200000045151,"Chain","Supply only stainless steel chain 6mm grade 40 to exhibit a higher tensile strength.","Per meter",30,"R","R"]
["H2.14",3036644,"Chain and 50mm Padlock","Supply and install stainless steel chain 6mm grade 40 to exhibit a higher tensile strength.","Per meter",30,"R","R"]
["H2.15",3035264,"Swimming lane anchors","Supply and replace stainless steel eyebolt & raw bolt M10.","Per item",30,"R","R"]
["H2.16",200000045152,"Storage drums for swimming lanes","Supply only a complete and robust steel construction galvanized storage drum on trolly suitable for 100m of 100mm Ø lane ropes.","Per item",10,"R","R"]
["H2.17",200000045153,"Cover for storage drums","Supply only a UV protective covers for storage drums suitable for 100m ropes.","Per item",10,"R","R"]
["H3",null,"STARTING BLOCKS  "]
["H3.1",3035265,"Fina type starting blocks 500 x 500 platform, all fibreglass construction including numbers on 4 sides. Distance above deck level 330mm.","Supply and replace with chemical anchors.","Per item",10,"R","R"]
["H3.2",3035266,"Fina type starting blocks 500 x 500 platform, all fibreglass construction including numbers on 4 sides. Distance above deck level 440mm.","Supply and replace with chemical anchors.","Per item",10,"R","R"]
["H3.3",3035267,"Fina type starting blocks 500 x 500, Stainless steel suitable for EDT wiring.","Supply and replace with chemical anchors.","Per item",10,"R","R"]
["H3.4",3035268,"Starting blocks for standard pools, 340 x 400 fibreglass","Supply and replace with chemical anchors.","Per item",10,"R","R"]
["H3.5",3035269,"Starting blocks for standard pools, 400 x 450 fibreglass","Supply and replace with chemical anchors.","Per item",10,"R","R"]
["H3.6",3036645,"Top surface of starting platform","Supply and replace with non-slip coating of starting platform start surface.","m2",10,"R","R"]
["H3.7",3035270,"Repair starting block replacing 4 chemical anchors","Supply and replace 4 -8mm bolts & nuts stainless steel with chemical anchor and mixing nozzle.","Per item",10,"R","R"]
["H4",null,"LADDERS"]
["H4.1",3035271,"Ladder, 2 step Stainless steel","Supply and replace 2 step stainless steel ladder minimum 38mm pipe size, with in-deck sleeves for holding ladder, easily removable.","Per item",10,"R","R"]
["H4.2",3035272,"Ladder, 3 step Stainless steel","Supply and replace 3 step stainless steel ladder minimum 38mm pipe size, with in-deck sleeves for holding ladder, easily removable.","Per item",10,"R","R"]
["H4.3",3035273,"Ladder, 4 step Stainless steel","Supply and replace 4 step stainless steel ladder minimum 38mm pipe size, with in-deck sleeves for holding ladder, easily removable.","Per item",10,"R","R"]
["H4.4",3036646,"Ladder, repair existing step stainless steel","Supply and repair by welding steps per joint Ø 50/38/16mm.","Per item",10,"R","R"]
["H5",null,"HEAT PUMPS & BLANKETS",null,null," "]
["H5.1",3035274,"Solar cover (per m2)","Supply and replace solar cover (e.g. 400 Micron reinforced Geobubble Solar weave) Weight per m² ± 368gms, bubble width & length 15 x 30mm, bubble height 5,5mm, Number of bubble per m²  ± 1943.","m2",500,"R","R"]
["H5.2",3036647,"Solar cover patch kit","Supply and repair with solar cover patch kit.","Per kit",10,"R","R"]
["H5.3",200000045163,"Roll up stations with UV protected cover for blankets","Supply only a new roll up station. Stands: Constructed 80 x 40 x 1.5mm 304 stainless steel, Height 730mm, Width 600mm Tubes: aluminium minimum of 127mm Ø wall thickness 3,5mm with reinforcing. Tubes be naturally anodised against corrosion, Fittings: Nylon fittings must be UV stabilised, and glass filled for extra strength, Castors: swivel with brakes - 125mm Ø galvanised.","Per item",3,"R","R"]
["H5.4",3035275,"Heat pump with defrost cycle","Supply and replace stainless steel heat pump 220V, 1 phase 50Hz, minimum input 1.725kw, heat output 8.9kw. Water flow 120l p/min.","Per item",3,"R","R"]
["H5.5",3035276,"Heat pump with defrost cycle","Supply and replace stainless steel heat pump 380V, 3 phase 50Hz, minimum input 5.4kw, heat output 25kw. Water flow 120l p/min.","Per item",3,"R","R"]
["H5.6",3035277,"Heat pump with defrost cycle","Supply and replace stainless steel heat pump 380V, 3 phase 50Hz, minimum input 6.5kw, heat output 40kw. Water flow 120l p/min.","Per item",3,"R","R"]
["H5.7",3035279,"EW55 Electrode Hot Water Boiler","Supply and service - complete service on EW55 Electrode Hot Water Boiler. Includes the replacement of packings. Insulator gaskets and sleeves. Heat Exchanger. Electrical Parts Insulator Clamps and Bolts. Retorque electrode assembly and tighten gland after 24hrs operation.","Per item",3,"R","R"]
["H5.8",3035280,"EW55 Electrode Hot Water Boiler","Supply and service - Strip and clean 2 x PTL  90 heat exchangers.","Per item",3,"R","R"]
["H5.9",3036648,"Water Treatment","Supply and service - Electro Boiler Solution EBS-01 20 ℓ.","Per item",3,"R","R"]
["H5.10",3036649,"Conductivity Prope","Supply and replace conductivity prope ¾ inch thread to monitor water treatment.","Per item",3,"R","R"]
["H5.11",3035278,"Dosing Pump","Supply and replace dosing pump to regulate water treatment 230VAC suction height 1.5m.","Per item",1,"R","R"]
["H5.12",200000045166,"Pool Thermometer floating (monitoring pool loop temperature)","Supply and replace - thermometer 0°C -60°C temperature gauge with ½ inch thread & 100mm stem and bulb well.","Per item",3,"R","R"]
["H5.13",200000045167,"Pool Thermometer for the boiler loop, e.g. Hillcrest Swimming Pool","Supply and replace - thermometer 0°C -120°C temperature gauge with ½ inch thread & 100mm stem and bulb well.","Per item",3,"R","R"]
["H5.14",3036650,"Pressure Gauge","Supply and replace - pressure gauge 0 – 100kpa  10mm thread.","Per item",3,"R","R"]
["H5.15",3036651,"Pressure Gauge","Supply and replace - pressure gauge 0 – 250kpa 10mm thread.","Per item",3,"R","R"]
["Total for Category H (Excluding VAT)",{"$nulls":6},"R"]
[]
["I  1",null,"EQUIPMENT, CHEMICALS AND POOL CARE ETC"]
["I 1.1",200000045170,"Equipment - Hi - VAC Brush/sweeper","Supply only a new complete unit Hi - VAC pool brush/sweeper head with fittings. Dimensions: 250 x 55 x 170mm","Per item",25,"R","R"]
["I 1.2",200000045836,"Equipment – replacement for Hi - VAC Brush/sweeper","Supply only a new replacement brush unit for Hi - VAC pool brush/sweeper. Dimensions: 250 x 55 x 170mm","Per item",10,"R","R"]
["I 1.3",200000037976,"Equipment - Pool Pole Aluminium 5m","Supply only a 5m Aluminium pole with stainless steel bolts and nuts.  Pole wall thickness must be no less than 1.1mm thick, with anodised finish to enhances durability and resistance to corrosion. The pole end must be designed for use with various pool cleaning attachments with easily switch out attachments for versatile cleaning solutions.","Per item",25,"R","R"]
["I 1.4",200000045171,"Equipment – Pool Leaf rake","Supply only Leaf rake for pools with a heavy-duty frame, nylon net with fine mesh netting for efficient debris removal and must easily connect to most standard pool poles for extended reach. Frame dimensions: Height 430mm Length 500mm Width 30mm","Per item",25,"R","R"]
["I 1.5",200000045172,"Equipment – pool Leaf rake De lux","Supply only Leaf rake De lux (Large) for pools with a scoop front design on frame, large, deep nylon net with fine mesh netting and must easily connect to most standard pool poles. Frame dimensions: Height  435mm Length 510mm Width 55mm","Per item",25,"R","R"]
["I 1.6",200000045173,"Equipment - 150mm Nylon brush","Supply only Nylon pool wall brush 150mm that must easily connect to most standard pool poles. Height 50mm Length 150mm","Per item",25,"R","R"]
["I 1.7",200000045174,"Equipment - 150mm Stainless steel brush","Supply only a stainless-steel pool brush with a 150mm compact head. Refer to 3.1 Specification details","Per item",25,"R","R"]
["I 1.8",200000045175,"Equipment – 450 mm Nylon brush","Supply only Nylon pool wall brush 450mm with curved design that must easily connect to most standard pool poles. Length 460mm Width 170mm Height 55mm","Per item",25,"R","R"]
["I 1.9",200000045176,"Equipment - 250mm Stainless-steel pool brush","Supply only a stainless-steel pool brush with a 250mm compact head. Refer to 3.1 Specification details","Per item",25,"R","R"]
["I 1.10",200000045177,"Equipment - 38 mm suction / vacuum hose with hose connectors","Supply only commercial grade 15 m x 38 mm pool suction / vacuum hose that is designed to provide excellent reach and flexibility. Refer to 3.1 Specification details","Per item",25,"R","R"]
["I 1.11",200000045178,"Equipment – 63 mm floating flexible hose","Supply only a 20 m x 63 mm floating flexible hose for connecting water tanks to pumps. Refer to 3.1 Specification details","Per item",25,"R","R"]
["I 1.12",200000045179,"Equipment - 80mm floating flexible hose","Supply only 20 m x 80 mm floating flexible hose medium duty.  Refer to 3.1 Specification details","Per item",25,"R","R"]
["I 1.13",200000045180,"Water Testing 25 Strips","Supply only 4-Way Test Strips for Swimming Pools, 25 strips with a minimum shelf life of 24 months. Test strips must test the four essential water quality factors: Free Chlorine, pH, Total Alkalinity, and Cyanuric Acid (Stabilizer).","Per item",25,"R","R"]
["I 1.14",200000045181,"Water Testing 50 Strips","Supply only 4-Way Test Strips for Swimming Pools, 50 strips with a minimum shelf life of 24 months. Test strips must test the four essential water quality factors: Free Chlorine, pH, Total Alkalinity, and Cyanuric Acid (Stabilizer).","Per item",25,"R","R"]
["I 1.15",200000045834,"Water Testing Test strips","Supply only 4-in 1 pool water Test Kit with a minimum shelf life of 24 months. Test kit must test the four essential water quality factors: Free Chlorine, pH, Total Alkalinity, and Cyanuric Acid (Stabilizer).","Per kit",25,"R","R"]
["I 1.16",200000045835,"Water Testing Kit refill","Supply only Refills for 4-in 1 Test Kit compatible with kit in use and with a minimum shelf of 24 months. Test kit must test the four essential water quality factors: Free Chlorine, pH, Total Alkalinity, and Cyanuric Acid (Stabilizer).","Per kit",25,"R","R"]
["I 1.17",200000045182,"Mobile suction sweeper trolley","Supply only electro-plated trolley with 4 x 300 mm wheels and turntable table. Length 1500 mm x 760 mm wide and 500mm high that can take a load of 650Kg","Per item",25,"R","R"]
["I 1.18",3035281,"Suction equipment attached on sweeper trolley","Supply and replace on the trolly a 4-bag sand filter with 1Kw 220V swimming pool pump. Weatherproof electric switch and 30 m 2.5 mm core cabtire electrical cable. 30 m x 38 mm suction hose.","Per item",25,"R","R"]
["I 1.19",200000045183,"8 Wheel manual vacuum sweeper","Supply only a new smooth-rolling 8-wheel sweeper with 45º plastic adapter that can fit the 38 mm coupling. All wheels must be fitted with seal case bearings for smooth operation and commercial use.  The pole connection must be a swivel head connection. ","Per item",10,"R","R"]
["I 1.20",200000045184,"12 Wheel manual vacuum sweeper","Supply only a new smooth-rolling 12-wheel sweeper with 45º plastic adapter that can fit the 38 mm coupling. All wheels must be fitted with seal case bearings for smooth operation and commercial use.  The pole connection must be a swivel head connection.","Per item",15,"R","R"]
["I 1.21",200000045185,"Crawling Suction Cleaner","Supply only a new complete automatic crawling suction side pool cleaner with an adjustable regulator valve, 36 fin disc and 5m piping included.","Per item",10,"R","R"]
["I 1.22",200000045186,"Industrial Sweeper  ","Supply only an Industrial stainless steel pool sweeper with 680mm x 480mm fiberglass reinforced wheels and brushes with drag ropes.","Per item",1,"R","R"]
["I 1.23",3036660,"Temporarily Balk Pool Water storage","Supply and service - 10 000ℓ Water Bladder to empty pool into and refill afterwards. Storage per day.","10 000ℓ  ",15,"R","R"]
["I 1.24",3036661,"Temporarily Balk Pool Water storage","Supply and service - 15 000ℓ Water Bladder to empty pool into and refill afterwards. Storage per day.","15 000ℓ",10,"R","R"]
["I 1.25",3035282,"Temporarily Balk Pool Water storage","Supply and service - 50 000ℓ Water Bladder to empty pool into and refill afterwards. Storage per day.","50 000ℓ",5,"R","R"]
["I 1.26",3036662,"Labelling of equipment","Replace all labelling on equipment with durable, weather-resistant laminated label black on white minimum fond size 15mm.","Per meter",30,"R","R"]
["I  2",null,"CHEMICALS"]
["I 2.1",200000032992,"Celite 545 RV ","Supply only 20kg bags of higher-grade, lab-certified product Clite 545 RV flux-calcined diatomaceous earth with small uniform particles size ranges (20–40 microns)","20kg",100,"R","R"]
["I 2.2",200000032993,"Sodium carbonate (Soda Ash) Dense","Supply only 25kg bags of soda ash dense to raise pH in water treatment with no less than 0.9 g/cc (gram per cubic centimetre). The chemical must quickly increase the pH if water is too acidic (<7.2), must works fast and must increases alkalinity a little.","25kg",1500,"R","R"]
["I 2.3",200000037967,"Sodium Bicarbonate","Supply only 25kg bags to raise total alkalinity in pool water, which will help to stabilize water against sudden pH swings (buffering), prevent corrosion of metal fixtures and pool equipment. It must be safe to add in larger doses without overshooting pH.","25kg",15,"R","R"]
["I 2.4",200000032994,"Aluminium Sulphate Metal Free","Supply only 25kg bags of Aluminium Sulphate metal free water treatment grade flocculant that will improve water clarity by binding fine suspended particles. Heavy metals like Pb, Cd, Cr, Hg, As should be ≤ 0.001 % each (trace levels only).","25kg",700,"R","R"]
["I 2.5",200000046118,"Sodium Dichloroisocyanuric Acid (SDIC) stabilized granular chorine","Supply only 25kg containers of stabilized granular chlorine compound, with a pH of 6, containing approximately 60% available chlorine. It must disinfect pool water by releasing hypochlorous acid (active chlorine) while the built-in stabilizer (cyanuric acid) protects the chlorine from being destroyed by sunlight, making it a longer lasting chlorine treatment for outdoor pool sanitation.","25kg",700,"R","R"]
["I 2.6",200000046117,"Sodium Dichloroisocyanuric Acid (SDIC) stabilized granular chorine","Supply only 50kg containers of stabilized granular chlorine compound, with a pH of 6, containing approximately 60% available chlorine. It must disinfect pool water by releasing hypochlorous acid (active chlorine) while the built-in stabilizer (cyanuric acid) protects the chlorine from being destroyed by sunlight, making it a longer lasting chlorine treatment for outdoor pool sanitation.","50kg",700,"R","R"]
["I2.7",200000046119,"Inline Sodium Dichloroisocyanuric Acid (SDIC)  dispenser.","Supply and install an inline Sodium Dichloroisocyanuric Acid (SDIC)  dispenser to regulate the flow of the stabilized granular chorine into the swimming pool.  The refill capacity of the dispenser should be 100 kg."]
["I2.8",200000046120,"Swimming pool water quality monitor ","Supply and activate a water quality monitor need to be able to measure key water metrics such as pH, chlorine and temperature. The smart devise must have capabilities to notify/ alert users when chemicals are needed to be added to the swimming pool."]
["I 2.9",200000046121,"Trichloroisocyanuric Acid (TCCA). Stabilized chlorine tablets.","Supply only 25kg containers of stabilized steady, slow release (chlorine is bound to an isocyanurate stabilizer) chlorine tablets with a pH: 2.7 - 3.3. ","25kg",200,"R","R"]
["I 2.10",200000046122,"Trichloroisocyanuric Acid (TCCA). Stabilised chlorine tablets.","Supply only 50kg containers of stabilized steady, slow release (chlorine is bound to an isocyanurate stabilizer) chlorine tablets with a pH: 2.7 - 3.3.","50kg",200,"R","R"]
["I 2.11",200000032996,"Filter media, 40 kg bags","Supply only Silica Sand 0.4 -1.6mm Ø.","per item",400,"R","R"]
["I 2.12",200000046123,"Hydro anthracite, 40 kg bags","Supply only 40kg of certified black, hard, angular granules of hydro anthracite water filter media with common grades of 0.8–1.4 mm or 1.0–2.0mm.","per item",25,"R","R"]
["I 2.13",200000037968,"Hydrochloric Acid (pool acid)","Supply only a 5ℓ hydrochloric acid with no less than 30% hydrochloric acid concentrate for reducing pH and total alkalinity in swimming pool and spa water.","5 litres",100,"R","R"]
["I 2.14",200000045187,"Hydrochloric Acid (pool acid)","Supply only a 25ℓ hydrochloric acid with no less than 30% hydrochloric acid concentrate for reducing pH and total alkalinity in swimming pool and spa water.","25 litres",100,"R","R"]
["I 2.15",200000037970,"Ammonia 250mm","Supply only a 250ml bottle of ammonia used for detecting Chlorine gas leaks.","250ml",100,"R","R"]
["I  3",null,"ONCE WEEKLY POOL WATER AND SYSTEM MAINTENANCE SERVICE"]
["I 3.1",3035283,"Once a week pool water and system maintenance","Supply and service - clean pool and filtration equipment service as per point 3.5.","50m x 25m pool",25,"R","R"]
["I 3.2",3035284,"Once a week pool water and system maintenance","Supply and service - clean pool and filtration equipment service as per point 3.5.","25m x 20m pool",25,"R","R"]
["I 3.3",3035345,"Once a week pool water and system maintenance","Supply and service - clean pool and filtration equipment service as per point 3.5.","0,4m x Ø6m Baby pool",25,"R","R"]
["I 3.4",3035285,"Once a week pool water and system maintenance","Supply and service - clean pool and filtration equipment service as per point 3.5.","1.4m x Ø7m Slide Pool",25,"R","R"]
["I 3.5",3035286,"Once a week pool water and system maintenance","Supply and service - clean pool and filtration equipment service as per point 3.5.","25m x 8m x 1,4m training pool",25,"R","R"]
["I 3.6",3035287,"Once a week pool water and system maintenance","Supply and service - clean pool and filtration equipment service as per point 3.5.","0,6m x Ø10m Splash pool",25,"R","R"]
["I 3.7",3036663,"Vertical Water Tank 5 000ℓ","Supply and replace 5 000ℓ vertical water tank diameter not more than 1850mm to fit on base stand.","per item",10,"R","R"]
["I 3.8",3036664,"Vertical Water Tank 10 000ℓ","Supply and replace 10 000ℓ vertical water tank diameter not more than 2200mm to fit on base stand.","per item",10,"R","R"]
["I 3.9",3036665,"Vertical Tank Stand 5 000ℓ","Supply and replace high-grade steel structure designed by engineers, strong enough to hold the entire weight of full tank of water. Floor space 2300mm x 2300mm 1,5m high.","per item",10,"R","R"]
["I 3.10",3036666,"Vertical Tank Stand 10 000ℓ","Supply and replace high-grade steel structure designed by engineers, strong enough to hold the entire weight of full tank of water. Floor space 3000mm x 3000mm 3m high.","per item",10,"R","R"]
["Total for Category I (Excluding VAT)",{"$nulls":6},"R"]
[]
["J1",null,"ADMINISTRATION AND TRAINING"]
["J1.1",3030111,"Training per trainee","Supply - On-the-job training service to swimming pool staff Training program should including evaluation and attendance certificate with a minimum of 3 hours per day x 2 days per training. Daily support for 8 x continuing weeks of remote monitoring (WhatsApp or other apps) with advice on daily dosing of the pool. (See paragraph 3.3 Training Plan)","Per trainee",35,"R","R"]
["J1.2",3035288,"Fault finding Inspection and Report (excluding point 3.8.1 (d), (e) and (f)","Supply and service a 50m x 25m pool - Inspection per swimming Pool with written report.","50m x 25m pool",30,"R","R"]
["J1.3",3035289,"Fault finding Inspection and Report (excluding point 3.8.1 (d), (e) and (f)","Supply and service a 25m x 20m pool - Inspection per swimming Pool with written report.","25m x 20m pool",30,"R","R"]
["J1.4",3035290,"Fault finding Inspection and Report (excluding point 3.8.1 (d), (e) and (f)","Supply and service a 0,4m x Ø6 Baby pool - Inspection per swimming Pool with written report.","0,4m x Ø6 Baby pool",30,"R","R"]
["J1.5",3035291,"Fault finding Inspection and Report (excluding point 3.8.1 (d), (e) and (f)","Supply and service a 1,4m x Ø7m Slide pool - Inspection per swimming Pool with written report.","1,4m x Ø7m Slide pool",30,"R","R"]
["J1.6",3035292,"Fault finding Inspection and Report (excluding point 3.8.1 (d), (e) and (f)","Supply and service a 25m x 8m x 1,4m training pool - Inspection per swimming Pool with written report.","25m x 8m x 1,4m training pool",30,"R","R"]
["J1.7",3035293,"Fault finding Inspection and Report (excluding point 3.8.1 (d), (e) and (f)","Supply and service a 0,6m x Ø10 Splash pool - Inspection per swimming Pool with written report.","0,6m x Ø10 Splash pool",30,"R","R"]
["J1.8",3035294,"Fault finding Inspection and Report (excluding point 3.8.1 (d), (e) and (f)","Supply and service the Filtration Plant - Inspection per swimming Pool with written report.","Filtration Plant",30,"R","R"]
["J1.9",3035295,"Transport / Travel cost","TRAVEL COSTS\nTravelling distance will be calculated from Tshwane House towards respective areas and back. Include cost for the completion of delivery or work @ R/km.","Per Purchase order\n(Assume to be \n100 km for evaluation purposes only).",100,"R                    /km","R"]
["J1.10",3030113,"Strip and Quote","Strip and provide quotation as per J1.10","per item",100,"R","R"]
["Total for Category J (Excluding VAT)",{"$nulls":6},"R"]
[]
["K1",null,"AFTER HOURS CALL OUT FOR THEFTS, BREAKDOWNS AND INCIDENTS (TBI) FOR UNPLANNED REPAIRS OR  A FORCES OF NATURE\n","After hours start from arriving on site after 17h00 to 09h00 of the next day, including  weekends and public holidays. Response time must be within 3 hours from receiving the emergency call out."]
["K1.1",3035296,"After hours from arriving on site (Attach proof of call out request and time sheet) Labour Artisan.","Call out - only applicable for after hour emergency work, i.e. Thefts, Breaks, Incidents or act of nature. (See table 3.1).","Per Hour",100,"R","R"]
["K1.2",3035297,"After hours from arriving on site  Labour - Skilled.","Call out - only applicable for after hour emergency work, i.e. Thefts, Breaks, Incidents or act of nature. (See table 3.1).","Per Hour",100,"R","R"]
["K1.3",3035298,"After hours arriving on site (Attach proof of call out request and time sheet)  Labour – Unskilled.","Call out - only applicable for after hour emergency work, i.e. Thefts, Breaks, Incidents or act of nature. (See table 3.1).","Per Hour",100,"R","R"]
["Total for Category K (Excluding VAT)",{"$nulls":6},"R"]
[]
["L1",null,"MISCELLANEOUS"]
["L1.1","N.A","Proven cost of material or spares not specified on the tender (actual quotation from a reputable service provider (registered on the NT Central Supplier Database or hold a valid TAX clearance certificate from SARS).","Attach a quotation from a reputable service provider from which the items will be sourced.  On request the project manager may request 3 quotations. (See table 3.1).","Assume material or spares cost R1 000 for evaluation purposes. (The R1000 will be replaced with the amount on the actual quote after appointment)",1,"R1 000 \n(Illustration purposes)","R1 000 \n(Illustration purposes)"]
["L1.2","N.A","Mark-up % on proven cost of material or spares not specified on tender ","Indicate the mark-up on handling fee for items not specified in this tender. Labour included.","Percentage mark-up should not exceed 15% (maximum).",1,"Assume material cost R1 000 for evaluation purposes.\nR 1 000 X \n\n\n___________  %","R"]
["Total for Category L (Excluding VAT)",{"$nulls":6},"R"]
[]
[]
[]
["SUMMARY "]
["Item Number",null,"ITEM DESCRIPTION",{"$nulls":4},"TOTAL AMOUNT\nEXCLUDING VAT"]
["A",null,"Total for Category A",{"$nulls":4},"R"]
["B",null,"Total for Category B",{"$nulls":4},"R"]
["C",null,"Total for Category C",{"$nulls":4},"R"]
["D",null,"Total for Category D",{"$nulls":4},"R"]
["E",null,"Total for Category E",{"$nulls":4},"R"]
["F",null,"Total for Category F",{"$nulls":4},"R"]
["G",null,"Total for Category G",{"$nulls":4},"R"]
["H",null,"Total for Category H",{"$nulls":4},"R"]
["I",null,"Total for Category I",{"$nulls":4},"R"]
["J",null,"Total for Category J",{"$nulls":4},"R"]
["K",null,"Total for Category K",{"$nulls":4},"R"]
["L",null,"Total for Category L",{"$nulls":4},"R"]
[{"$nulls":6},"SUB TOTAL ","R"]
[{"$nulls":6},"VAT ","R"]
[{"$nulls":6},"TOTAL ","R"]