{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["A&B Schedules","Deviation Schedule","Test Schedule","Drawing"],"not_rendered":{"external_links":2,"defined_names":4},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"A&B Schedules","index":0,"n_rows":59,"n_cols":7,"rows_kept":59,"merged":[[0,0,0,6],[1,1,1,6],[2,1,2,6],[3,1,3,6],[4,0,4,6],[5,2,5,4],[5,5,5,6],[6,2,6,4],[6,5,7,6],[7,2,7,4],[8,1,8,6],[10,1,10,6],[11,1,11,6],[14,2,14,3],[15,2,15,3],[16,3,16,4],[22,3,22,4],[31,2,31,4],[32,2,32,5],[33,3,33,4],[35,3,35,4],[39,3,39,4],[47,0,47,6],[48,1,49,6],[51,0,51,6],[53,0,53,1],[58,2,58,3]],"flags":["formulas_cached_only"]}
["ESKOM TENDER E2719DXLIMOU"]
[null,"Technical Schedules A and B for"]
[null," D-DT-3132 FERRULE, TINNED COPPER CU SEALING FERRULE 12MM LG SAP:165792"]
[null,"NB. UNIQUE SCHEDULES ARE TO BE COMPLETED PER SAP NUMBER LISTED BELOW "]
["NB. SUPPLIERS TO CONFIRM ADHERENCE TO THE LATEST PUBLISHED REVISION OF ALL APPLICABLE ESKOM DRAWINGS"]
[null,"Sap Number","Description",null,null,"SANS Specification"]
[null,229555,"SEAL TOOL-LESS BLUE D3132"]
[]
[null,"Note: the type test report shall be in accordance with SANS 61238-1, however the type test report based on NRS can be accepted with stated deviations on deviation schedule"]
[]
[null,"Schedule A:  Purchasers specific requirements"]
[null,"Schedule B:  Guarantees and technical particulars of equipment offered"]
[]
[null,1,null,2,null,3,4]
[null,"Item ","Description",null,"Requirements","Schedule A","Schedule B"]
[null,1,"Product Information"]
[null,1.1,"·","Purchasing details"]
[null,"1.1.1",null,"Eskom SAP No (Select from the drop down)",229555,"xxxxxxxxxx"]
[null,"1.1.2",null,"Manufacturer","Manufacturer name","xxxxxxxxxx"]
[null,"1.1.3",null,"Manufacturer's Product Code","Specify Code","xxxxxxxxxx"]
[null,"1.1.4",null,"Manufacturer's Drawing number & Revision number","Specify No and Rev","xxxxxxxxxx"]
[null,"1.1.5",null,"Manufacturer's physical unique identifier and knurl marks indelibly marked on product body","Specify markings","xxxxxxxxxx"]
[null,2,"·","Compliance to Eskom Buyer's Guide Drawings"]
[null,2.1,null,"FERRULE TINNED COPPER"," Eskom DDT-3132 ","YES"]
[null,"2.2",null,"SIZE : "," Eskom DDT-3132 (SAP 165792)","YES"]
[null,"2.2.1",null,"Diameter (Outside)","4 mm","YES"]
[null,"2.2.2",null,"Diameter (Inside)","2 mm","YES"]
[null,"2.2.3",null,"Length","12mm","YES"]
[null,"2.3.1",null,"Packaging","Supplied in clear plastic bag","YES"]
[null,"2.3.2",null,"Number of ferrules per pack",100,"YES"]
[null,"2.3.3",null,"(UMC,each)","1 Ferrule","YES"]
[null,3,"Documentation (to be submitted with tender)"]
[null,null,"Note:  All documentation to also be provided in electronic format."]
[null,"3.1","·","General"]
[null,"3.1.1",null,"Approved Manufacturer Drawings showing markings and dimensions","1 Set submitted","YES"]
[null,"3.2","·","Test Reports (Iin accordance with SANS 50483- 4,5 and 6)",null,"Required"]
[null,"3.2.1",null,"Has the relevant signed mandatory test schedule been submitted.","Signed Test Schedule Submitted ","YES"]
[null,"3.2.2",null,"Approved Manufacturing Drawing with revision number and history.","Specify","YES/NO"]
[null,"3.2.3",null,"Type test in accordance to 61238-1.","Signed Test Report Submitted ","YES/NO"]
[null,4,null,"Packaging"]
[null,"4.1",null,"Individually sealed ","each","Individually sealed "]
[null,"4.2",null,"Corrosion and mechanical damage protection",null,"Yes/No"]
[null,"4.3",null,"Information to appear on a bulk package\n• the name of the manufacturer;\n• the fitting reference and size;\n• the number of fittings per package;\n• the purchaser's order number; and\n• The date of manufacture.\n",null,"Yes"]
[null,"4.4",null,"Packaging material, method and maximum quantity, not exceeding 30kg.",null,"Supplier to provide details"]
[null,"4.5",null,"Markings to be stipulated.",null,"Supplier to provide details"]
[null,"4.6",null,"Installation instructions provided in packaging.",null,"YES"]
[]
["ESKOM TENDER E2719DXLIMOU"]
[null,"Deviations to any of the stated requirements are to be captured on the Deviation Schedule."]
[]
[]
["SUPPLIER SIGNATURES"]
[]
[null,null,"         "]
[{"$nulls":3},"Name (Print)",null,"Company name"]
[]
[]
[]
[null,null,"Sign",null,null,"Date"]

{"sheet":"Deviation Schedule","index":1,"n_rows":46,"n_cols":6,"rows_kept":46,"merged":[[0,0,0,6],[1,0,1,6],[2,0,2,6],[3,0,3,6],[4,0,4,6],[5,2,5,6],[6,2,6,6],[7,2,7,6],[8,2,8,6],[9,2,9,6],[10,2,10,6],[11,2,11,6],[12,2,12,6],[13,2,13,6],[14,2,14,6],[15,2,15,6],[16,2,16,6],[17,2,17,6],[18,2,18,6],[19,2,19,6],[20,2,20,6],[21,2,21,6],[22,2,22,6],[23,2,23,6],[24,2,24,6],[25,2,25,6],[26,2,26,6],[27,2,27,6],[28,2,28,6],[29,2,29,6],[30,2,30,6],[31,2,31,6],[32,2,32,6],[33,2,33,6],[34,2,34,6],[35,2,35,6],[37,0,37,6],[38,0,38,6],[40,0,40,1],[41,2,41,3],[45,2,45,3]],"flags":["formulas_cached_only"]}
["ESKOM TENDER E2719DXLIMOU"]
["Deviation schedule"]
[" D-DT-3132 FERRULE, TINNED COPPER CU SEALING FERRULE 12MM LG SAP:165792"]
["SAP No: 229555"]
["Any deviations offered to this specification shall be listed below with reasons for deviation.  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective that that specified by Eskom."]
["Item","Clause","Description of Deviation"]
{"$rows_empty":31}
["ESKOM TENDER E2719DXLIMOU"]
["SUPPLIER SIGNATURES"]
[]
[null,null,"         "]
[null,null,"Name (Print)",null,null,"Company name"]
[]
[]
[]
[null,null,"Sign",null,null,"Date"]

{"sheet":"Test Schedule","index":2,"n_rows":30,"n_cols":6,"rows_kept":30,"merged":[[0,0,0,6],[1,0,1,7],[2,0,2,7],[3,1,3,5],[4,0,4,7],[8,1,8,5],[13,2,13,5],[19,1,19,5],[21,1,21,8],[22,1,22,8],[25,1,25,2],[29,1,29,2]],"flags":["formulas_cached_only"]}
["ESKOM TENDER E2719DXLIMOU"]
["Test Report Schedule"]
[" D-DT-3132 FERRULE, TINNED COPPER CU SEALING FERRULE 12MM LG SAP:165792"]
[null,"The test reports are required for the selected SAP number listed on this sheet."]
["SAP No: 229555"]
[]
[null,1,2,3,4,5]
[null,"Item ","Description","Standard","Clause ","Report No."]
[null,"Electrical"]
[null,1,"Installation","SANS 61238-1","6.1"]
[null,2,"Measurements","SANS 61238","6.2"]
[null,2.1,"Electrical resistance measurements","SANS 61238","6.2.1"]
[null,2.2,"Temperature measurements","SANS 61238","6.2.2"]
[null,3,"Heat cycle test"]
[null,3.1,"First heat cycle","SANS  50483-6","6.3.1"]
[null,3.2,"Second heat cycle","SANS  50483-6","6.3.2"]
[null,3.3,"Subsequent heat cycles","SANS  50483-6","6.3.3"]
[null,3.4,"Short-circuit tests","SANS  50483-6","6.3.4"]
[null,4,"Assessment of results","SANS  50483-6","6.4"]
[null,"Mechanical tests:"]
[null,5,"Method","SANS 50483-5","7.1"]
[]
[null,"SUPPLIER SIGNATURES"]
[]
[]
[null,"Name (Print)",{"$nulls":3},"Company name"]
[]
[]
[]
[null,"Sign",{"$nulls":3},"Date"]

{"sheet":"Drawing","index":3,"n_rows":15,"n_cols":3,"rows_kept":15,"merged":[[0,0,0,7],[1,0,1,7],[2,1,2,5],[3,0,3,7]],"flags":["formulas_cached_only"]}
["Buyers Guide Drawing"]
[" D-DT-3132 FERRULE, TINNED COPPER CU SEALING FERRULE 12MM LG SAP:165792"]
[null,"The test reports are required for the selected SAP number listed on this sheet."]
[]
[]
[null,null,"SAP MATERIAL No.: 0229555"]
[null,null,"SHORT DESCRIPTION: SEAL TOOL-LESS BLUE D3132"]
[null,null,"TECH. DESCRIPTION:"]
[null,null,"ESKOM APPROVED TOOL-LESS SEAL AS PER SPECIFICATION DST 34-749"]
[null,null,"COLOUR: BLUE"]
[null,null,"SEAL IDENTIFYERS: UNIQUE NUMBER + BARCODE + ESKOM LOGO"]
[null,null,"SUPPLIED IN CLEAR PLASTIC BAGS * 50 SEALS/PACK *"]
[null,null,"BAG SHALL INDICATE THE SERIAL NUMBER RANGE OF SEALS INCLUDED"]
[null,null,"TO BE USED FOR SUPPLY CUT-OFF PURPOSES"]
[null,null,"ESKOM DRAWING No. D-DT-3132 *"]