{"text_format":"3","workbook":"xls","n_sheets":9,"sheets":["NOTES","SCHEDULE1-FIXED CHARGES","SCHEDULE1- TIME RELATED","SCHEDULE2-SITE CLEARANCE","SCHEDULE3-PARAMETER FENCING","Breakdown of Item 3.1","SCHEDULE4-CLEARVu FENCING","Sum Opt1","MOS"],"not_rendered":{"external_links":1,"defined_names":23},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"NOTES","index":0,"n_rows":37,"n_cols":5,"rows_kept":37,"flags":["formulas_cached_only"]}
["Please read the following notes"]
[]
["Page format"]
["Please do not change any format of these schedules"]
[]
["Cross references"]
["Items highlighted in",null,null,"insert reference from particular specifications in tender document (then remove highlight)"]
["Provisional sums highlighted in",{"$nulls":3},"insert sum of money (then remove highlight)"]
[]
["Contingencies and Escalation"]
["Items highlighted in",null,null,"on the summary page - insert % for contingencies and escalation (then remove highlight)"]
[]
["Text in red"]
["Check if text/size/etc shown is correct for your project - if not correct - change to suit - if correct -  leave as is and colour text in \"black\" "]
[]
["Contract:  «NUMBER» "]
["Insert number of contract in the <number> portion on the first schedule \"A-P&G \"only - "]
["it will then outomatically be copied in all the other schedules"]
[]
["Schedule no's"]
["Insert the schedule number on the top of each schedule (block F8) only - the same schedule number will outomatically be copied "]
["to the end of each schedule"]
["Delete schedules not required"]
[]
["Item numbers"]
["Item numbers in column A will be generated outomatically from (block F8) - except if \"additional items\" are inserted"]
["When new items are inserted please insert new item numbers for these items - add \"a\" ,\"b\" type simbols to the previous numbers above each item"]
["Please do not change the \"formula's\" in the page number cells"]
[]
["Summary page"]
["Chose one of summary page types from the attached ones and complete the schedule numbers and descriptions"]
[]
["Logo's"]
["If required by the Employer - insert Employer \"logo\" together with Bigen logo - or - omit bigen logo and use only Employer logo"]
[]
["Carried forward/Brought forward insert"]
["Please insert these page break inserts at the end of each page (dotted line showing page breaks)"]

{"sheet":"SCHEDULE1-FIXED CHARGES","index":1,"n_rows":58,"n_cols":11,"rows_kept":58,"merged":[[5,0,6,0],[5,2,6,6],[5,7,6,7],[5,8,6,8]],"flags":["formulas_cached_only"]}
["Masilo: Refurbishment of sport facility (Fencing)"]
["Part C2:  Pricing Data"]
["Section A1:  Schedule of Quantities"]
["Provisional Sums and Prime Cost Items"]
[]
["Item","Payment","Description",{"$nulls":4},"Unit","Qty","Rate","Amount"]
[null,"Reference",{"$nulls":7},"(R)","(R)"]
[]
[null,null,"PRELIMINARY AND GENERAL"]
[]
[null,"A","FIXED CHARGE ITEMS"]
[]
[null,null,"Contractual ralated Documentation ",{"$nulls":4},"Sum",1]
[]
[null,1,"Site Establishment"]
[]
[null,"1.1","Contractor’s Yard Fencing (establish and maintain)",{"$nulls":4},"sum",1]
[]
[null,"1.2","Site Offices (establishment)",{"$nulls":4},"sum",1]
[]
[null,"1.3","Site Stores (establishment)",{"$nulls":4},"sum",1]
[]
[null,"1.4","Facilities and eating area for workers",{"$nulls":4},"sum",1]
[]
[null,"1.5","Security",{"$nulls":4},"sum",1]
[]
[null,"1.6","Contractor's Plant, Equipment & Tools (establishment)",{"$nulls":4},"sum",1]
[]
[null,"1.7","Project Signboard",{"$nulls":4},"sum",1]
[]
[null,"1.8","Removal of site establishment on completion of the contract",{"$nulls":4},"sum",1]
[null,null,"as per EMP"]
[]
[null,2,"Health & Safety (OHS Act, Construction Regulations)"]
[]
[null,null,"Personal protective equipment :"]
[]
[null,"2.1","Hard hats",{"$nulls":4},"sum",1]
[]
[null,"2.1","Safety goggles or shields",{"$nulls":4},"sum",1]
[]
[null,"2.3","Gloves",{"$nulls":4},"sum",1]
[]
[null,"2.4","Safety shoes",{"$nulls":4},"sum",1]
[]
[null,"2.5","Overalls",{"$nulls":4},"sum",1]
[]
[null,"2.6","Compliance with safety plan & safety file",{"$nulls":4},"sum",1]
[]
[null,"2.7","Compliance with Covid-19 Regulations",{"$nulls":4},"PC sum",1,{"v":10000,"d":"10,000.00"}]
[]
[null,"2.8","Accredited Technical Training",{"$nulls":4},"PC sum",1,{"v":80000,"d":"80,000.00"}]
[]
[null,"2.10","Provision of Standards and Specifications",{"$nulls":4},"PC sum",1,{"v":30000,"d":"30,000.00"}]
[]
[null,2.11,"Handling cost and profit in respect subitem 2.10",{"$nulls":4},"%",{"v":10,"d":"10.00"},{"v":3000,"d":"3,000.00"}]
[]
[null,null,"Carried forward to Summary of Schedules",{"$nulls":6},"Total"]

{"sheet":"SCHEDULE1- TIME RELATED","index":2,"n_rows":81,"n_cols":11,"rows_kept":81,"merged":[[5,0,6,0],[5,2,6,6],[5,7,6,7],[5,8,6,8]],"flags":["formulas_cached_only"]}
["Masilo: Refurbishment of sport facility (Fencing)"]
["Part C2:  Pricing Data"]
["Section A1:  Schedule of Quantities"]
["Provisional Sums and Prime Cost Items"]
[]
["Item","Payment","Description",{"$nulls":4},"Unit","Qty","Rate","Amount"]
[null,"Reference",{"$nulls":7},"(R)","(R)"]
[]
[null,null,"PRELIMINARY AND GENERAL"]
[]
[null,"B","TIME RELATED ITEMS"]
[]
[null,null,"Contractual ralated Documentation ",{"$nulls":4},"Month",3]
[]
[null,null,"Programme and Planning"]
[]
[null,null,"Contractors must allow for the preparation of a detailed ",{"$nulls":4},"weeks",12]
[null,null,"programme reflecting the outage dates. "]
[]
[null,3,"Site establishment maintenance, etc."]
[]
[null,"3.1","Site Offices (maintain)",{"$nulls":4},"weeks",12]
[]
[null,"3.2","Site Stores (maintain)",{"$nulls":4},"weeks",12]
[]
[null,"3.3","Food and Accommodation of Employees",{"$nulls":4},"weeks",12]
[]
[null,"3.4","Contractor's Plant, Equipment & Tools (maintain)",{"$nulls":4},"weeks",12]
[]
[null,"3.5","Ablution Facilities",{"$nulls":4},"weeks",12]
[]
[null,"3.6","Water Supplies",{"$nulls":4},"weeks",12]
[]
[null,"3.7","Electricity Supplies",{"$nulls":4},"weeks",12]
[]
[null,"3.8","Communications (telephones)",{"$nulls":4},"weeks",12]
[]
[null,"3.9","Contractor's insurance (insurance payments and statutory",{"$nulls":4},"weeks",12]
[null,null,"contributions, provide certificates)"]
[]
[null,"3.10","Security (24 hours) - Actual Cost + 10%",{"$nulls":4},"weeks",12]
[]
[null,"3.11","Legal appointments in terms of the OHS Act and"]
[null,null,"Regulations.(Additional appointments,not part of workforce):"]
[]
[null,"3.11(a)","Construction Manager or alternate - Construction",{"$nulls":4},"weeks",12]
[null,null,"Regulations Clause 8 (1)"]
[]
[null,"3.11(b)","Health and Safety Officer (Full time / Part time) -",{"$nulls":4},"weeks",12]
[null,null,"Construction Regulations Clause 8 (5)&(6)"]
[]
[null,"3.11(c)","Construction supervisor. (Full time / Part time) -",{"$nulls":4},"weeks",12]
[null,null,"Construction Regulations Clause 8 (7) (Compulsory to list"]
[null,null,"the name of supervisor for the duration of contract in part 3,"]
[null,null,"paragraph 4)."]
[]
[null,"3.11 (d)","Storeman (Full time / Part time)",{"$nulls":4},"weeks",12]
[]
[null,"3.12","Other Health and Safety items deemed necessary to",{"$nulls":4},"sum",1]
[null,null,"comply to OHS Act, Regulations and Eskom Safety"]
[null,null,"specifications, Covid-19"]
[]
[null,"3.13","Health and Safety Representive (On site)",{"$nulls":4},"months",3]
[]
[null,"3.14","Community Liason Officer renumeration @ R5500/month",{"$nulls":4},"months",3]
[]
[null,"3.15","Project Steering Committee Cost @ R300 per sitting",{"$nulls":4},"months",3]
[]
[null,"3.16","Civil Engineering Trainee Student @ R7000/month",{"$nulls":4},"months",3]
[]
[null,"3.17","Handlingcostand profit in respect of subitem (3.14), (3.15), (3.16)"]
[]
[]
[null,"C","4. Environmental Management"]
[]
[null,"SANS","4.1 Compliance to Environmental Management Plan",{"$nulls":4},"weeks",12]
[]
[null,"D","5. Civil"]
[]
[null,"SANS","5.1 Compliance to Site Management Plan ",{"$nulls":4},"weeks",12]
[null,null,"Carried forward to Summary of Schedules",{"$nulls":6},"Total"]

{"sheet":"SCHEDULE2-SITE CLEARANCE","index":3,"n_rows":62,"n_cols":11,"rows_kept":62,"merged":[[5,0,6,0],[5,2,6,6],[5,7,6,7],[5,8,6,8]],"flags":["formulas_cached_only"]}
["Masilo: Refurbishment of sport facility (Fencing)"]
["Part C2:  Pricing Data"]
["Section C:  Schedule of Quantities"]
["VO-Extra Works"]
[]
["Item","Payment","Description",{"$nulls":4},"Unit","Qty","Rate","Amount"]
[null,"Reference",{"$nulls":7},"(R)","(R)"]
[]
[2,null,"SCHEDULE: 2"]
[null,null,"SITE CLEARANCE"]
[]
[]
[]
[2.1,"2.1.1","The Contractor shall completely, remove, transport and dump",{"$nulls":4},"m",600]
[null,null,"at a registered dumping site which shall be identified by the"]
[null,null,"Municipality Engineer Representative , all existing  trees and"]
[null,null,"shrubs which are in the way of new perimeter wall, "]
[null,null,"guardhouse and ablution building. (2m wide)"]
[]
[null,"2.1.2","The Contractor shall completely, remove, transport and dump",{"$nulls":4},"m",0,"rate only"]
[null,null,"at a registered dumping site which shall be identified by the"]
[null,null,"Municipality Engineer Representative , all demolished existing"]
[null,null,"fences which are in the way of new perimeter wall."]
[]
[null,"2.1.3","The Contractor shall  barricade at all excavations, fenceline",{"$nulls":4},"m",600]
[null,null,"bordering resident houses or intervering with gravesites, "]
[null,null,"positions and material type to be confirmed on site by"]
[null,null,"Municipality Engineer Representative."]
[]
[null,"2.1.4","The Contractor shall completely, remove, transport and",{"$nulls":4},"m",160]
[null,null,"dumped at a registered dumping site which shall be located  "]
[null,null,"by the Municipality, all topsoil to a depth of 150mm and 2m"]
[null,null,"wide from centre of foundation."]
[]
[2.2,null,"REINFORCEMENT"]
[]
[null,"2.2.1","The Contractor shall completely, supply, transport and install",{"$nulls":4},"Ton",1.44]
[null,null,"reinforcement (binding wire and 50mm spacers included) as"]
[null,null,"indicated on the drawing for the wall.  Refer to drawing :"]
[]
[3,null,"SURVEY"]
[]
[null,3.1,"The Contractor shall locate (peg) the position of the new fence",{"$nulls":4},"PC Sum",1,{"v":35000,"d":"35,000.00"}]
[null,null,"guardhouse and ablution buildings,  using a registered land"]
[null,null,"surveyor"]
[]
[null,3.2,"The Contractor shall provide all survey equipment, assistants",{"$nulls":4},"PC Sum",1,{"v":10000,"d":"10,000.00"}]
[null,null,"and markers using a registered land surveyor"]
[]
[null,3.3,"The Contractor shall compile as-built drawings for the position",{"$nulls":4},"PC Sum",1,{"v":20000,"d":"20,000.00"}]
[null,null,"of the new perimeter fence and buildings including"]
[null,null,"co-ordinates."]
[]
[null,3.4,"Overhead Charges to Item 3.1,3.2 and 3.3",{"$nulls":4},"%",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"}]
[]
[]
[]
[]
[null,null,"SCHEDULE: 2"]
[null,null,"SITE CLEARANCE"]
[]
[null,null,"Carried forward to Summary of Schedules",{"$nulls":6},"Total"]

{"sheet":"SCHEDULE3-PARAMETER FENCING","index":4,"n_rows":62,"n_cols":11,"rows_kept":62,"merged":[[5,0,6,0],[5,2,6,6],[5,7,6,7],[5,8,6,8]],"flags":["formulas_cached_only"]}
["Masilo: Refurbishment of sport facility (Fencing)"]
["Part C2:  Pricing Data"]
["Section B:  Schedule of Quantities"]
["Parameter Fencing"]
[]
["Item","Payment","Description",{"$nulls":4},"Unit","Qty","Rate","Amount"]
[null,"Reference",{"$nulls":7},"(R)","(R)"]
[]
[3,"SABS 1200A","SCHEDULE: 3"]
[null,null,"PARAMETER FENCING "]
[]
[3.1,"PCC-4.1",null,"Brick Wall fencing (1.8m high) according to ",{"$nulls":3},"m",310]
[{"$nulls":3},"specification including excavations, "]
[{"$nulls":3},"foundation concreting, posts, pales and ground "]
[{"$nulls":3},"beams. All as per drawing."]
[]
[3.2,"PCC-4.1",null,"Supply and install according to specification a 6m",{"$nulls":3},"No",1]
[{"$nulls":3}," wide vehicular gate"]
[]
[3.3,"PCC-4.1",null,"Supply and install according to specification 1.5m ",{"$nulls":3},"No",2]
[{"$nulls":3},"wide pedestrian gate as per drawing"]
[]
[3.4,"PCC-4.1",null,"Contractor shall source supply and transport all ",{"$nulls":3},"m",610]
[{"$nulls":3},"fence and galvinised painting for intermediate and"]
[{"$nulls":3},"corner post support 600mm high for a new "]
[{"$nulls":3},"600dia razor wire"]
[]
[]
[4,null,"BUILDINGS"]
[]
[null,null,"Construct the security guardhouse complete as per drawing"]
[null,null,"including earthworks, foundation excavations, importation of",{"$nulls":4},"m²",9]
[null,null,"material under surface bed, concrete for foundations and"]
[null,null,"surface bed, cladding and sheeting, brickwork, roofing,"]
[null,null,"waterproofing, carpentry and joinery, ironmongery, windows,"]
[null,null,"burglar door & bars, doors and frames, plastering, tiling,"]
[null,null,"sanitary fittings, cold water supply pipes fittings, sewer"]
[null,null,"connection. As indicated on the drawing."]
[]
[5,null,"Warning Signs"]
[]
[null,null,"Supply, transport and install the following signs and"]
[null,null,"notices to the Sports complex fence, gates and buildings",{"$nulls":7},"`"]
[]
[null,5.1,"Unauthorized Entry",{"$nulls":4},"no.",4]
[]
[null,5.2,"Sports complex Identity",{"$nulls":4},"no.",4]
[]
[null,5.3,"Ablution identification signs",{"$nulls":4},"no.",3]
[]
[null,5.4,"Prohibitive Construction entry (various)",{"$nulls":4},"no.",4]
{"$rows_empty":7}
[null,null,"SCHEDULE: 3"]
[null,null,"PARAMETER FENCING "]
[]
[null,null,"Carried forward to Summary of Schedules",{"$nulls":6},"Total"]

{"sheet":"Breakdown of Item 3.1","index":5,"n_rows":69,"n_cols":11,"rows_kept":69,"merged":[[5,0,6,0],[5,2,6,6],[5,7,6,7],[5,8,6,8]],"flags":["formulas_cached_only"]}
["Masilo: Refurbishment of sport facility (Fencing)"]
["Part C2:  Pricing Data"]
["Section B:  Schedule of Quantities"]
["Parameter Fencing"]
[]
["Item","Payment","Description",{"$nulls":4},"Unit","Qty","Rate","Amount"]
[null,"Reference",{"$nulls":7},"(R)","(R)"]
[]
[3.1,"SABS 1200A","SCHEDULE: 3.1"]
[null,null,"PARAMETER FENCING "]
[]
["3.1.1","PCC-4.1","The Contractor shall completely, excavate the trenches for the",{"$nulls":4},"m³",57.599999999999994]
[null,null,"foundation fence and the guardhouse and ablution block."]
[null,null,"As indicated on the drawing."]
[]
[null,null,"The Contractor shall spoil all excess material on site to the",{"$nulls":4},"m³",54]
["3.1.2","PCC-4.1","registered land fill site or as indicated by the Municipality"]
[null,null,"Engineer Representative.. (within a radius of 20km)"]
[]
["3.1.3","PCC-4.1","The Contractor shall import G6 material  and compact 150mm",{"$nulls":4},"m³",130]
[null,null,"layers to fill the holes where trees were removed, excess"]
[null,null,"material shall be used for guardhouse and ablution block"]
[]
["3.1.4","PCC-4.1","The Contractor shall import dump-rock to deal with discovered",{"$nulls":4},"m³",9.332999999999998]
[null,null,"underground water"]
[]
["3.1.5","PCC-4.1","The Contractor shall compact in situ and G6 material to 93%",{"$nulls":4},"m³",220]
[null,null,"MOD ASSHTO."]
[]
[3.2,null,"CONCRETE WORKS"]
[]
["3.2.1",null,"The Contractor shall completely, supply, transport and",{"$nulls":4},"m²",155]
[null,null,"install rough wooden/steel shutters where necessary to"]
[null,null,"complete the works."]
[]
["3.2.2",null,"The contractor shall completely, supply, transport, cast and",{"$nulls":4},"m³",1.037]
[null,null,"float No-Fine Concrete to deal with discovered undergraound"]
[null,null,"water"]
[]
["3.2.3",null,"The Contractor shall completely, supply, transport, float",{"$nulls":4},"m³",45.25]
[null,null,"and cast concrete 25MPa/19 for the boundary fence."]
[null,null,"Supply concrete test results for every 10m3 casted or 60m."]
[]
[3.3,null,"BRICK WORKS"]
[]
["3.3.1",null,"Brick Wall fencing (1.8m high)",{"$nulls":4},"m",310]
{"$rows_empty":19}
[null,null,"SCHEDULE: 3.1"]
[null,null,"PARAMETER FENCING "]
[]
[null,null,"Carried forward to Summary of Schedules",{"$nulls":6},"Total"]

{"sheet":"SCHEDULE4-CLEARVu FENCING","index":6,"n_rows":187,"n_cols":11,"rows_kept":187,"merged":[[5,0,6,0],[5,2,6,6],[5,7,6,7],[5,8,6,8]],"flags":["formulas_cached_only"]}
["Masilo: Refurbishment of sport facility (Fencing)"]
["Part C2:  Pricing Data"]
["Section C:  Schedule of Quantities"]
["ClearVu Fencing"]
[]
["Item","Payment","Description",{"$nulls":4},"Unit","Qty","Rate","Amount"]
[null,"Reference",{"$nulls":7},"(R)","(R)"]
[]
[4,null,"SCHEDULE: 4"]
[null,null,"CLEARVu FENCING"]
[]
[null,null,"HIGH SECURITY FENCES & GATES CLEAR Vu OR "]
[null,null,"SIMILAR APPROVED"]
[null,null,"References Codes and Standards"]
[null,null,"A. SANDF ROP OV1, CSIR TEST 980289 050036 050056 "]
[null,null,"T09998, SABS 2536/YM, North Atlantic Treaty Organization "]
[null,null,"(NATO) 5660-99-371 - 1515"]
[]
[4.1,null,"SUPPLY AND ERECTION OF FENCING:",{"$nulls":4},"m",300]
[null,"4.1.1","1.8m High ClearVu Fence OR Similar approved – "]
[null,null,"Galvanized"]
[]
[null,null,"a) Taper Post: "]
[{"$nulls":3},"- Post shall be 3m long Taper Post of 85mm x 85mm "]
[{"$nulls":3},"x 45mm one piece without joints."]
[{"$nulls":3},"- Post shall include ‘Locking Recess Mechanism’ to  "]
[{"$nulls":3},"secure panel edge. "]
[{"$nulls":3},"- Post shall be sealed with a UV stabilized polymer cap."]
[{"$nulls":3},"- Post shall be Hot Dipped Galvanized after fabrication "]
[{"$nulls":3},"whereby zinc coating shall be smooth and essentially "]
[{"$nulls":3},"free from lumps, globs, or points. "]
[]
[null,null,"b)  Panel : "]
[{"$nulls":3},"- Panel shall be 1.8m in height and a width of 3.382m"]
[{"$nulls":3},"- Panel aperture size shall be 76.2 mm x 12.7 mm "]
[{"$nulls":3},"- Mesh panel steel pressed with 4 x v-bends (rigidity), "]
[{"$nulls":3},"2 x 70 degree side flanges (all internal fixtures – "]
[{"$nulls":3},"shielded from attack) and top and toe bend made up "]
[{"$nulls":3},"of high carbon wire in accordance to BS EN 10223-4.  "]
[{"$nulls":3},"- Tensile strength of welds must be at least 75% of the"]
[{"$nulls":3}," tensile strength of the wire as per SABS 2536/YM139,"]
[{"$nulls":3}," 8 x anti-scale gussets positioned where bend "]
[{"$nulls":3},"connects to."]
[{"$nulls":3},"- Panel shall be affixed to post over 48 line wires using "]
[{"$nulls":3},"8 x Double bolt comb clamps and 8 x Single bolt comb "]
[{"$nulls":3},"clamps with 24 x Anti vandal tech bolt. "]
[{"$nulls":3},"- Panel shall be Hot Dipped Galvanized, then Alu-galv "]
[{"$nulls":3},"coated"]
[{"$nulls":3},"- Panel shall be Hot Dipped Galvanized, then Alu-galv "]
[{"$nulls":3},"coated"]
[{"$nulls":3},"- Coating shall be corrosion tested by CSIR salt spray "]
[{"$nulls":3},"for 1008 hours without signs of red rust."]
[]
[null,null,"c) Topping: "]
[{"$nulls":3},"- 100mm Castle Spike rail secured to 50mm wide "]
[{"$nulls":3},"Clearvu mesh flange bent along fence top."]
[]
[null,null,"Finish: Galvanized."]
[]
[]
[]
[{"$nulls":9},"Carried Forward"]
[{"$nulls":9},"Brought Forward"]
[]
[]
[null,null,"INSTALLATION"]
[]
[null,null,"a) General "]
[{"$nulls":3},"- Install all fencing and gates in accordance with the "]
[{"$nulls":3},"drawings, specifications and manufactures instruction.  "]
[]
[null,null,"b) Cement"]
[4.2,null,null,"- High strength concrete shall be used and suitable for "]
[null,"4.2.1",null,"footings and foundations. (typically 400mm x 400mm "]
[{"$nulls":3},"x 600mm)"]
[{"$nulls":3},"- Should the foundation used in soils containing high "]
[{"$nulls":3},"sulphate levels, concrete made with special "]
[{"$nulls":3},"sulphate-cement shall be used."]
[{"$nulls":3},"- High Strength Concrete shall be used within "]
[{"$nulls":3},"30 minutes of adding water. Concrete should be fully"]
[{"$nulls":3}," compacted before finishing."]
[]
[null,null,"c) Posts "]
[{"$nulls":3},"- Taper posts shall be spaced at intervals of 3.382 m. "]
[{"$nulls":3},"- Post holes shall be cleared of loose material.  Waste "]
[{"$nulls":3},"material shall be spread where directed by Engineer. "]
[{"$nulls":3},"- The ground surface irregularities along the fence line "]
[{"$nulls":3},"shall be eliminated to the extent necessary "]
[{"$nulls":3},"- Posts shall be set plumb, and follow the indicated "]
[{"$nulls":3},"alignment.  All posts shall be set to the depth indicated"]
[{"$nulls":3},"on the design documents. "]
[{"$nulls":3},"- Concrete shall be thoroughly consolidated around "]
[{"$nulls":3},"each post, free of voids, and finished with a domed "]
[{"$nulls":3},"shaped surface, with the base of dome at grade "]
[{"$nulls":3},"elevation."]
[{"$nulls":3},"- Concrete shall be allowed to cure prior to installing "]
[{"$nulls":3},"any additional components to the posts. "]
[{"$nulls":3},"- Concrete footings and continuous sill shall be carried "]
[{"$nulls":3},"down to at least the depth indicated on the design "]
[{"$nulls":3},"documents and shall not be smaller than the "]
[{"$nulls":3},"dimensions shown.  Posts shall be approximately "]
[{"$nulls":3},"centered in their footings.  All concrete shall be placed "]
[{"$nulls":3},"promptly and consolidated by tamping or other "]
[{"$nulls":3},"approved methods.  All excess material from footings,"]
[{"$nulls":3}," including loose material used for curing, shall be "]
[{"$nulls":3},"disposed of as directed by the Engineer."]
[{"$nulls":3},"- Longer posts should be applied to areas of severe  "]
[{"$nulls":3},"gradient. "]
{"$rows_empty":15}
[{"$nulls":9},"Carried Forward"]
[{"$nulls":9},"Brought Forward"]
[]
[]
[null,null,"d) Panel"]
[{"$nulls":3},"- On the ground, position 70 degree panel flange "]
[{"$nulls":3},"against internal side of taper post ensuring a flush "]
[{"$nulls":3},"post/panel finish. Place single clamps, double clamps "]
[{"$nulls":3},"and anti-scale gussets as per design documents. "]
[{"$nulls":3},"- Tech bolt drilled through until fastened. Repeat "]
[{"$nulls":3}," process on other side once panel/post has been lifted"]
[{"$nulls":3}," into position.   "]
[]
[null,null,"e) Gates "]
[{"$nulls":3},"- Gates shall be installed at the locations shown. "]
[{"$nulls":3}," Hinged gates shall be mounted to swing as indicated."]
[4.3,null,null,"-  Latches, stops, and keepers shall be installed as"]
[{"$nulls":3}," required. "]
[null,"4.3.1",null,"- Adjust gate to operate smoothly, easily, and quietly, "]
[{"$nulls":3},"free from binding, warp, excessive deflection, distortion, "]
[{"$nulls":3},"nonalignment, misplacement, disruption, or "]
[{"$nulls":3},"malfunction, throughout entire operational range.  "]
[{"$nulls":3},"- Confirm that latches and locks engage accurately and "]
[{"$nulls":3},"securely without forcing or binding. "]
[{"$nulls":3},"- Lubricate hardware and other moving parts."]
[]
[{"$nulls":3},"- Security gates Diamond mesh",{"$nulls":3},"No",1]
[]
[{"$nulls":3},"- Steel Double Gate",{"$nulls":3},"No",1]
[]
[{"$nulls":3},"- Steel Single Gate",{"$nulls":3},"No",2]
[]
[{"$nulls":3},"- Security gates Razor wire and Razor Ribbon Coils",{"$nulls":3},"No",1]
[]
[null,null,"INSIDE FENCING (DIAMOND MESH)"]
[]
[null,null,"a) Supply & erect of 50 x 50 x 2.5 mesh and 500mm razor ",{"$nulls":4},"m",550]
[null,null,"flatwrap wire coils to detail including all excavation, "]
[null,null,"backfilling and hot dipped galvanising."]
[]
[null,null,"b) Supply & erect 100mm diam. x 3mm MS  pole in ",{"$nulls":4},"No",65]
[null,null,"straining post, gate post and corner post inc. concrete "]
[null,null,"bases and supply & erect 60mm diam. X 3mm MS anchor"]
[null,null," poles and concrete bases."]
[]
[null,null,"c) Double vehicle entrance gate complete with chain, ",{"$nulls":4},"No",1]
[null,null,"hinges and barrel bolts as per detail drawing 3.0m wide"]
[]
[null,null,"d) Supply and install according to specification a 6m wide ",{"$nulls":4},"No",1]
[null,null,"vehicular gate"]
[]
[null,null,"e) Supply and install according to specification 1.5m wide ",{"$nulls":4},"No",2]
[null,null,"pedestrian gate as per drawing"]
{"$rows_empty":7}
[null,null,"SCHEDULE: 4"]
[null,null,"CLEARVu FENCING"]
[]
[null,null,"Carried forward to Summary of Schedules",{"$nulls":6},"Total"]

{"sheet":"Sum Opt1","index":7,"n_rows":42,"n_cols":7,"rows_kept":42,"merged":[[5,0,5,2],[6,0,6,2],[7,0,7,2],[8,0,8,2],[9,0,9,2],[10,0,10,2],[32,0,32,1],[33,0,33,1],[34,0,34,1],[35,0,35,1],[36,0,36,1]],"flags":["formulas_cached_only"]}
["Masilo: Refurbishment of sport facility (Fencing)",{"$nulls":5},"a"]
["Part C2:  Pricing Data",{"$nulls":5},"b"]
["Part C2:  Pricing Data",{"$nulls":5},"c"]
["Section C2.3: Summary of Schedules",{"$nulls":5},"d"]
[]
["Masilonyana Local Municipality"]
["Theunissen"]
["CONTRACT: "]
["Masilo: Refurbishment of sport facility (Fencing)"]
[]
[" Summary of Schedules"]
[]
["Schedule No.","Description","Amount ( R )"]
[1,"SCHEDULE1-PRELIMINARY AND GENERAL"]
[2,"SCHEDULE2-SITE CLEARANCE"]
[3,"SCHEDULE3-PARAMETER FENCING"]
[4,"SCHEDULE4-CLEARVu FENCING"]
{"$rows_empty":15}
["Sub-Total"]
["Provisional sum: Allowance for Contingencies (10% of Sub-Total)",{"$nulls":3}," "]
["Total Construction Cost"]
["Value Added Tax at 15%"]
["Total Amount due "]
[]
["Signature :"]
["By Tenderer :"]
["Company Name :"]
["Date :"]

{"sheet":"MOS","index":8,"n_rows":52,"n_cols":9,"rows_kept":52,"merged":[[0,0,0,8],[1,0,2,8],[3,0,3,8],[4,0,4,1],[4,3,4,8],[5,0,5,1],[5,3,5,8],[6,0,6,1],[6,3,6,8],[7,0,7,1],[7,3,7,8],[8,0,8,1],[8,3,8,8],[9,0,9,1],[9,3,9,8],[10,0,10,1],[10,3,10,6],[11,0,11,8],[12,0,12,8],[13,0,14,0],[13,1,14,4],[13,5,14,5],[13,6,13,7],[13,8,14,8],[15,1,15,4],[16,1,16,4],[17,1,17,4],[18,1,18,4],[19,1,19,4],[20,1,20,4],[21,1,21,4],[22,1,22,4],[22,11,22,15],[23,1,23,4],[23,11,23,15],[24,1,24,4],[24,11,24,15],[25,1,25,4],[26,1,26,4],[27,1,27,4],[28,1,28,4],[29,1,29,4],[30,1,30,4],[31,1,31,4],[32,1,32,4],[33,1,33,4],[34,1,34,4],[35,1,35,4],[36,1,36,4],[37,1,37,4],[38,1,38,4],[39,1,39,4],[40,1,40,4],[41,1,41,4],[42,0,42,7],[43,0,43,7],[44,0,44,8],[45,0,45,8],[46,0,46,8],[47,0,47,8],[48,0,48,8],[49,0,49,7],[50,0,50,7],[51,0,51,8],[52,0,52,8],[53,0,53,7],[54,0,54,7]],"flags":["formulas_cached_only"]}
[]
["MATERIALS ON SITE"]
[]
[]
["Name of Service",null,":","Masilo: Refurbishment of sport facility (Fencing)"]
[]
["Contract No",null,":","2022/08/004"]
[]
["Date",null,":","2024-02-09"]
[]
["Contractor",null,":",{"$error":"#REF!"},{"$nulls":3},"Certificate No.  :",{"v":3,"d":" 3"}]
[]
[]
["No.","Description",{"$nulls":3},"Rate","Quantity",null,"Amount"]
[{"$nulls":6},"Previous","Present"]
{"$rows_empty":27}
["Net Amount of Material on Site",{"$nulls":7},{"v":0,"d":"  R  0.00"}]
["80 % of Material on Site",{"$nulls":7},{"v":0,"d":"  R  0.00"}]
[]
["Notes:"]
["1.     Unless marked all material orders are not subject"]
["         to contract price adjustment"]
["2.      Following items are not included :"]
["         a)   Main contractor's discount"]
["         b)   Main contractor's profit and attendance"]
["         c)   15 %  V A T"]