{"text_format":"3","workbook":"xlsx","n_sheets":17,"sheets":["Addendum 3 - Cover","Addendum 3 - Clarifications","Addendum 2 - Cover","Addendum 2 - Clarifications","Cover Sheet","Technical Clarifications","Valve Data - All Sites","Acacia Power Station","Ankerlig Power Station","Drakensberg Pumped Storage","Gariep Hydro Power Station","Gourikwa OCGT Power Station","Ingula Pumped Storage Scheme","Palmiet Pumped Storage","Port Rex Gas Turbine","Sere Wind Farm","Vanderkloof Hydro Power"],"not_rendered":{"images":12,"defined_names":11},"read":"whole","date_system":"1900"}

{"sheet":"Addendum 3 - Cover","index":0,"n_rows":48,"n_cols":2,"rows_kept":48,"merged":[[47,0,47,3]]}
["VALVE DATA PACKAGE - TENDER ADDENDUM"]
["TENDER E2979GXPOU"]
["Supply and Delivery of Various Valves and Valve Components for Peaking Power Stations"]
["ADDENDUM NO. 3"]
[]
["ADDENDUM DETAILS"]
["Issue Date:","2026-09-04"]
["Revision:",3]
["Status:","ISSUED FOR TENDER"]
[]
["TENDER EXTENSION NOTICE"]
["Original Closing Date:","2026-07-02"]
["Extended Closing Date:","2026-09-17"]
[]
["SCOPE OF THIS ADDENDUM"]
["This addendum contains additional technical clarifications received from site end-users at various Peaking Power Stations in response to bidder queries."]
[]
["DOCUMENTS INCLUDED IN THIS ADDENDUM"]
["1. Technical Clarifications 3","25 items with site feedback (22 complete, 3 awaiting information)"]
[]
["SUMMARY OF CLARIFICATIONS"]
["Sites with clarifications:","Drakensberg PSS, Ingula PSS, Palmiet PSS"]
["Items clarified:",22]
["Items awaiting information:",3]
["Information provided:","OEM/Brand, Part Numbers, Pressure Classes, Technical Specifications, Serial Numbers"]
[]
["REFERENCE DOCUMENTS"]
["• Invitation to Tender (ITT) E2979GXPOU"]
["• Attachment 4 - Price List and Item Descriptions"]
["• Attachment 5 - Eskom Standard Conditions of Tender (30 January 2025)"]
["• Technical Clarifications (Revision 1 & 2)"]
[]
["IMPORTANT NOTES TO BIDDERS"]
[]
["Partial Quotations:","Permitted per ITT Clause 1.6 and Eskom Standard Conditions of Tender Clause 1.6. Eskom reserves the right to accept the whole or any specified part of the tender."]
[]
["Bidder Response Options:"]
["• QUOTED","Compliance with specifications (technical datasheet required)"]
["• NOT QUOTING","Item not within bidder's product range"]
["• INSUFFICIENT DATA","Unable to quote; submit RFI through official channels"]
[]
["Technical Information:","Complete technical information may not be available for all items. Bidders may exclude items from their submission without prejudice to their overall tender."]
[]
["Award Structure:","Award may be to one or multiple suppliers on a line-item or category basis."]
[]
["Evaluation:","Per ITT Clauses 2.22 (no alternatives), 3.13 (70% functionality threshold), 3.15 (90/10 preferential procurement)."]
[]
["All terms and conditions of the original Invitation to Tender E2979GXPOU and Eskom Standard Conditions of Tender (30 January 2025) remain in full force and effect."]

{"sheet":"Addendum 3 - Clarifications","index":1,"n_rows":36,"n_cols":8,"rows_kept":36,"merged":[[0,0,0,7],[1,0,1,7],[2,0,2,1],[2,2,2,3],[2,4,2,7],[29,0,29,7],[31,0,31,7],[32,0,32,7],[33,0,33,7],[34,0,34,7],[35,0,35,7]]}
["TENDER E2979GXPOU - OUTSTANDING INFORMATION FROM SITES - REVISION 3"]
[]
["Issue Date: 4 September 2026",null,"Revision: 3",null,"Status: ISSUED FOR TENDER"]
["No.","Site","Mat. No.","Description","OEM/Supplier","Supplier Question","Eskom Response","Status"]
[1,"Ingula Pumped Storage Scheme",721178,"VALVE, CHECK: TL34; 3 IN; DN80; 2 BAR; SERGI (FRANCE)","SERGI","OEM requires serial numbers of TP systems.","Ingula site response: TYPE: Check valve / non-return mechanical shutter; MODEL: TL34; SIZE: 3 IN / DN80 (80 mm nominal diameter); PRESSURE RATING: 2 bar differential pressure capacity; MANUFACTURER: SERGI; APPLICATION: Transformer conservator shutter valve; TEMPERATURE RATING: -40-100 DEG C; BODY MATERIAL: ALSI7MG0.65T685HBS; OPERATED: 250 VDC SUPPLY; NOTE: Nickel plated double door check valve style.","COMPLETE"]
[2,"Drakensberg Pumped Storage Scheme",738160,"VALVE, NRV NON RETURN: 1/2 IN; 16 BAR; SS 316; SERGI FRANCE","SERGI","OEM requires serial numbers of TP systems.","Drakensberg site response: VALVE: TYPE: NRV NON RETURN; VALVE SIZE: 1/2 IN; DESIGN RATING: 16 BAR; TEMPERATURE RATING: -198 TO 260 DEG C; CONNECTION: 1/2 IN; OPERATED: FLOW; BODY MATERIAL: STAINLESS STEEL 316; STYLE: 1 WAY; SOFTGOODS: GASKET; MANUF P/N: 111929400252002+00; REFERENCE NO: FTTPDS48E 01; SERGI FRANCE","COMPLETE"]
[3,"Drakensberg Pumped Storage Scheme",77169,"VALVE, GATE: 100 MM; SOLID WEDGE; FLANGE; STEEL; 150 LB; HYDRAULIC; RISING OS; BOLTED BONNET","Velan","Specifications not according to Velan. Request drawings, datasheets or pictures of valve tags.","Drakensberg site response: VALVE, GATE: VALVE SIZE: 100 MM; TYPE: SOLID WEDGE; CONNECTION: FLANGE; BODY MATERIAL: STEEL; TRIM: BONNET STL; OPERATED: HYDRAULIC; STEM DESIGN: RISING OUTSIDE SCREW; STYLE: BOLTED BONNET; DESIGN RATING: 150 LB; REFERENCE NO: 20WRC; RUNNER COOLING WATER SUPPLY AUTO","COMPLETE"]
[4,"Drakensberg Pumped Storage Scheme",77242,"VALVE, ANGLE: GLOBE; 100 MM; 600 LB; FLANGE; STL; HYDRAULIC; BOLTED BONNET","Velan","Specifications not according to Velan. Request drawings, datasheets or pictures of valve tags.","Drakensberg site response: VALVE, ANGLE: TYPE: GLOBE; VALVE SIZE: 100 MM; DESIGN RATING: 600 LB; CONNECTION: FLANGE; BODY MATERIAL: STL; OPERATED: HYDRAULIC; STYLE: BOLTED BONNET; TRIM: BONNET/STEM STL; DRAWING NO: M-6WO78AG8 REV 1; REFERENCE NO: 20DA1/2; AIR ADMISSION; FOR TAIL WATER DEPRESSING","COMPLETE"]
[5,"Ingula Pumped Storage Scheme",620391,"VALVE, GATE: 250 MM; ISOLATING; 2-2.8 MPA; FLANGE; STAINLESS STEEL; ACTUATOR; NON RISING; JIS 20K","Velan","Specifications not according to Velan. Request drawings, datasheets or pictures of valve tags.","[AWAITING SITE INFORMATION]","PENDING"]
[6,"Drakensberg Pumped Storage Scheme",640478,"VALVE, GLOBE: 2 IN; 102 BAR; FLANGE; A216 GR WCB; HANDWHEEL; CL 600","Velan","Specifications not according to Velan. Request drawings, datasheets or pictures of valve tags.","Drakensberg site response: VALVE, GLOBE: VALVE SIZE: 2 IN; DESIGN PRESSURE: 102 BAR; DESIGN TEMPERATURE: -29 TO 38 DEG C; FACE TO FACE LENGTH: 292.1 MM; OPERATED: HANDWHEEL, MANUAL; CONNECTION: FLANGE; BODY MATERIAL: A216 GR WCB; TRIM: A182F6; GRADE: A216 GR WCB; SOFTGOODS: PACKING GRAPHITE; STEM DESIGN: A182F6; APPLICATION: RUNNER SEAL ISOLATION; SPECIFICATION: CL 600; TYPE: ISOLATING; DESIGN RATING: ASME B19.34; TEMPERATURE RATING: ASME B16.34; CONNECTION ASME B16.5/B16.25; TESTING AND INSPECTION: API 598","COMPLETE"]
[7,"Drakensberg Pumped Storage Scheme",66523,"VALVE, GATE: 300 MM; SOLID WEDGE; FLANGE; STL CAST; HANDWHEEL GEAR; 100 BAR","Velan","Specifications not according to Velan. Request drawings, datasheets or pictures of valve tags.","Drakensberg site response: VALVE, GATE: VALVE SIZE: 300 MM; TYPE: SOLID WEDGE; CONNECTION: FLANGE; BODY MATERIAL: STL CAST; TRIM: BONNET STL; OPERATED: HANDWHEEL, GEAR; STEM DESIGN: RISING OS; STYLE: BOLTED BONNET; DESIGN RATING: 100 BAR; HYDRO TEST CERTIFICATE REQUIRED; REFER TO CONTRACT OPY 49218","COMPLETE"]
[8,"Drakensberg Pumped Storage Scheme",68910,"VALVE, GLOBE: 1/2 IN; BW; CS ASTM A105; HANDWHEEL; 2500 PSI; Y BODY","Velan","Specifications not according to Velan. Request drawings, datasheets or pictures of valve tags.","Drakensberg site response: VALVE, GLOBE: VALVE SIZE: 1/2 IN; OPERATED: HANDWHEEL; CONNECTION: BW; BODY MATERIAL: CS ASTM A105; TRIM: DISC/SEAT HF; STEM SS GR 410; STEM DESIGN: RISING SPINDLE; STYLE: INTEGRAL BONNET; Y BODY; DESIGN RATING: 2500 PSI; TEMPERATURE RATING: 840 DEG F; REFERENCE NO: 578; VELAN","COMPLETE"]
[9,"Drakensberg Pumped Storage Scheme",178437,"VALVE, NEEDLE: 6 IN; FLANGE; STL","Velan","Specifications not according to Velan. Request drawings, datasheets or pictures of valve tags.","Drakensberg site response: VALVE, NEEDLE: VALVE SIZE: 6 IN; CONNECTION: FLANGE; BODY MATERIAL: STL","COMPLETE"]
[10,"Ingula Pumped Storage Scheme",657955,"VALVE, FLAPPER: CHECK; DN80; FLANGE; STAINLESS STEEL; PN160","Velan","Specifications not according to Velan. Request drawings, datasheets or pictures of valve tags.","Ingula site response: VALVE TYPE: Check / Flapper (non-return valve); NOMINAL SIZE: DN80 (80 mm or 3-inch); END CONNECTION: Face flanges on both ends; MATERIAL: Stainless Steel (corrosion-resistant); PRESSURE RATING: PN160 (160 bar / 16,000 kPa / approx. Class 900 ANSI); APPLICATION: TURBINE; SPECIFICATION: ISO 9001; MANUF P/N: 4N602CL; MATERIAL GRADE: 1.4408","COMPLETE"]
[11,"Ingula Pumped Storage Scheme",620394,"VALVE, GATE: 1-1/2 IN; ISOLATING; FLANGE; A105; HANDWHEEL; JIS 10K","Velan","Specifications not according to Velan. Request drawings, datasheets or pictures of valve tags.","Ingula site response: TYPE: Gate valve; SIZE: 1-1/2 inch (DN40); BODY MATERIAL: ASTM A105 (standard forged carbon steel for high-temperature and ambient service); END CONNECTION: Flanged ends; PRESSURE RATING: JIS 10K (PN16-style capacity); OPERATION: Manual handwheel; TRIM: 13CR; STEM DESIGN: Rising; APPLICATION: Oil level; SPECIFICATION: API 602, RF style.","COMPLETE"]
[12,"Palmiet Pumped Storage Scheme",714976,"VALVE, PLUG: 80; PN40; CARBON STEEL; HYDRAULIC; COMPRESSED AIR BLOWDOWN","SchuF","Kindly provide nameplate for this item.","Palmiet site response: VALVE, PLUG: VALVE SIZE: 80; DESIGN RATING: PN40; TEMPERATURE RATING: -10 TO 100 CELSIUS; CONNECTION: THREADED CONNECTION (G1/2); BODY MATERIAL: CARBON STEEL; FACE TO FACE LENGTH: 155 MM; OPERATED: HYDRAULIC; SOFTGOODS: O-RING RUBBER 85X3 / O-RING RUBBER 102X3 / MANTEL-RING TFMA 90X88X7.3 / NUT-RINGB12X24X10 / SCRAPER-RING B12X22; CONFIGURATION: FLANGE; APPLICATION: COMPRESSED AIR; TYPE: BLOWDOWN; MANUF P/N: 2.49-581; MANUFACTURER: VOITH GMBH; NOTE: Supplier to contact Voith GmbH with Manufacturer Part Number 2.49-581. Reference drawing number 2.41-48230 for verification.","COMPLETE"]
[13,"Drakensberg Pumped Storage Scheme",66205,"VALVE, RELIEF: SET PRESSURE: 60 BAR; MB8-222-2450C60B; SAFETY","Maximator","Provide Maximator equipment model/serial number to verify correct parts.","Drakensberg site response: VALVE, RELIEF: SET PRESSURE: 60 BAR; REFERENCE NO: MB8-222-2450C60B; SAFETY","COMPLETE"]
[14,"Drakensberg Pumped Storage Scheme",77155,"VALVE, SOLENOID: 10 MM; 5 WAY; 220 VAC; 315 BAR; STEEL; OIL; S10G51G020001100","Maximator","Provide Maximator equipment model/serial number to verify correct parts.","Drakensberg site response: VALVE, SOLENOID: PIPE SIZE: 10 MM; STYLE: 5 WAY; POTENTIAL: 220 VAC; DESIGN RATING: 315 BAR; BODY MATERIAL: STEEL; MEDIUM: OIL; REFERENCE NO: S10G51G020001100; 35 HZ; CONNECTION MANIFOLD; GENERAL PURPOSE ENCLOSURE; PUMP PILOT VALVE","COMPLETE"]
[15,"Drakensberg Pumped Storage Scheme",77149,"VALVE, SOLENOID: 10 MM; 2/4 WAY; 220 VAC; 315 BAR; STEEL; GAS/LIQUID; S10G51 G019 011M","Maximator","Provide Maximator equipment model/serial number to verify correct parts.","Drakensberg site response: VALVE, SOLENOID: PIPE SIZE: 10 MM; STYLE: 2/4 WAY; POTENTIAL: 220 VAC; DESIGN RATING: 315 BAR; BODY MATERIAL: STEEL; MEDIUM: GAS/LIQUID; POWER: 34 W; REFERENCE NO: S10G51 G019 011M; MB9-642.8800; CONNECTION MANIFOLD; OPERATION SOLENOID; GENERAL PURPOSE ENCLOSURE","COMPLETE"]
[16,"Drakensberg Pumped Storage Scheme",77160,"VALVE, SOLENOID: 8 MM; 4 WAY; 220 VAC; 315 BAR; STEEL; GAS/LIQUID; S10G51G020061300","Maximator","Provide Maximator equipment model/serial number to verify correct parts.","Drakensberg site response: VALVE, SOLENOID: PIPE SIZE: 8 MM; STYLE: 4 WAY; POTENTIAL: 220 VAC; DESIGN RATING: 315 BAR; BODY MATERIAL: STEEL; OPERATED: SOLENOID; MEDIUM: GAS/LIQUID; POWER: 34 W; CAT NO: 52 012 31; REFERENCE NO: S10G51G020061300; CONNECTION MANIFOLD; GUIDE VANE TIMING CONTROL; 40 L/MIN; ENCLOSURE GENERAL PURPOSE","COMPLETE"]
[17,"Drakensberg Pumped Storage Scheme",77161,"VALVE, SOLENOID: 8 MM; 4/2 WAY; 220 VDC; STEEL; GAS/LIQUID; S10G51G0200","Maximator","Provide Maximator equipment model/serial number to verify correct parts.","Drakensberg site response: VALVE, SOLENOID: PIPE SIZE: 8 MM; STYLE: 4/2 WAY; POTENTIAL: 220 VDC; BODY MATERIAL: STEEL; MEDIUM: GAS/LIQUID; POWER: 34 W; REFERENCE NO: S10G51G0200; CONNECTION MANIFOLD; GENERAL PURPOSE ENCLOSURE; CONTROL","COMPLETE"]
[18,"Ingula Pumped Storage Scheme",637560,"VALVE, RELIEF: 1 IN; 88 BAR; G1 IN-BSPP; STAINLESS STEEL 316; AIR; COMPRESSOR; M33H03X00V56V66J23H01","Leser","Need model numbers to offer quotation.","Ingula site response: COMPONENT TYPE: Pressure relief valve; CONNECTION: 1 inch with G 1-inch BSPP threads; RELIEF PRESSURE: 88 bar; MATERIAL: Stainless Steel 316; MEDIA: Compressed air; MODEL NUMBER: M33H03X00V56V66J23H01; APPLICATION: BLW Compressors; PRESSURE RANGE: IN PN 250; OUT PN 40. NOTE: Verify material specification with BLW compressors.","COMPLETE"]
[19,"Ingula Pumped Storage Scheme",637562,"VALVE, RELIEF: 1/2 IN; 3 BAR; THD 1/2 IN; STAINLESS STEEL 316; AIR; COMPRESSOR; M33H03X00V54V65","Leser","Need model numbers to offer quotation.","Ingula site response: TYPE: Pressure relief valve; SIZE: 1/2 inch; SET PRESSURE: 3 bar; MATERIAL: Stainless Steel 316; APPLICATION: Air / Gas; PART IDENTIFIER: M33H03X00V54V65; PRESSURE RANGE: IN PN 250; OUT PN 160.","COMPLETE"]
[20,"Ingula Pumped Storage Scheme",660516,"VALVE, PILOT: 1 WAY; 6 MM; STL; GPFX730094P0001; ABB; FOR GEN CIRCUIT BREAKER","ABB","Kindly provide us with a picture of the valve.","Ingula site response: COMPONENT TYPE: Pilot Valve / Servo Valve; CONFIGURATION: 1-Way (Single-acting directional control); SIZE: 6 mm nominal diameter; MATERIAL: Steel (STL); PART NUMBER: GPFX730094P0001; MANUFACTURER: ABB; OPERATING VOLTAGE: 220-250 V DC; PRIMARY APPLICATION: Generator Circuit Breaker (GCB) operating mechanism. NOTE: This item is for C&I (Control & Instrumentation).","COMPLETE"]
[21,"Palmiet Pumped Storage Scheme",62312,"VALVE, SOLENOID: 10 MM; 4/2 WAY; 250 VAC; 315 BAR; STEEL; DC SOLENOID; AIR/LIQUID; S10G51G0230615MV; HERION","Herion","Please confirm with the customer the correct voltage of this valve - this is very important. The specifications ask for AC and DC.","Palmiet site response: VALVE, SOLENOID: PIPE SIZE: 10 MM; STYLE: 4/2 WAY; POTENTIAL: 250 VAC; DESIGN RATING: 315 BAR; CONNECTION: COMPRESSION; BODY MATERIAL: STL; OPERATED: DC SOLENOID; ENCLOSURE RATING: IP54; MEDIUM: AIR/LIQUID; POWER: 36 W; MANUF P/N: S10G51G0230615MV; CATALOGUE NO: 52051.9000; HERION DIRECTIONAL CONTROL VALVE; NOTE: Voltage confirmed as 250 VAC only - no DC voltage. Pressure test certificates to be supplied on delivery.","COMPLETE"]
[22,"Drakensberg Pumped Storage Scheme",63348,"VALVE, BALL: 3/4 IN; 1000 KPA; FEMALE THD; LEVER; 3 WAY; 3 PIECE; BALL SS GR 316; SEALS PTFE; CF8M; ACID WATER OIL AND GAS","Swagelok","Kindly advise what ratio/percentage is the acid water on your line, as well as the temperature.","[AWAITING SITE INFORMATION]","PENDING"]
[23,"Drakensberg Pumped Storage Scheme",205470,"KIT: SEALS; SPH/VALVE OPERATOR; ROOF TYPE LIP RING; SUPPORTING RING; THRUST RING; SIZE ID 250 X OD 280 MM","LIP","Please provide us with the nameplate and serial number of the valve. This will assist us in identifying the brand of the valve.","[AWAITING SITE INFORMATION]","PENDING"]
[24,"Ingula Pumped Storage Scheme",721178,"VALVE, CHECK: TL34; 3 IN; DN80; 2 BAR; SERGI (FRANCE)","SERGI","OEM requires completion of Quotation Processing Requirements form to prepare accurate offer. Sites to provide: transformer details, serial numbers, installation information, and operating conditions.","Ingula site response: TYPE: Check valve / non-return mechanical shutter; MODEL: TL34; SIZE: 3 IN / DN80 (80 mm nominal diameter); PRESSURE RATING: 2 bar differential pressure capacity; MANUFACTURER: SERGI; APPLICATION: Transformer conservator shutter valve; TEMPERATURE RATING: -40-100 DEG C; BODY MATERIAL: ALSI7MG0.65T685HBS; OPERATED: 250 VDC SUPPLY; NOTE: Nickel plated double door check valve style.","COMPLETE"]
[25,"Drakensberg Pumped Storage Scheme",738160,"VALVE, NRV NON RETURN: 1/2 IN; 16 BAR; SS 316; SERGI FRANCE","SERGI","OEM requires completion of Quotation Processing Requirements form to prepare accurate offer. Sites to provide: transformer details, serial numbers, installation information, and operating conditions.","Drakensberg site response: VALVE: TYPE: NRV NON RETURN; VALVE SIZE: 1/2 IN; DESIGN RATING: 16 BAR; TEMPERATURE RATING: -198 TO 260 DEG C; CONNECTION: 1/2 IN; OPERATED: FLOW; BODY MATERIAL: STAINLESS STEEL 316; STYLE: 1 WAY; SOFTGOODS: GASKET; MANUF P/N: 111929400252002+00; REFERENCE NO: FTTPDS48E 01; SERGI FRANCE","COMPLETE"]
["--- End of Clarifications ---"]
[]
["TENDER EXTENSION REQUEST"]
["Extended Closing Date: 17 September 2026 at 10:00 (SAST)"]
["Extension Notice: The tender closing date has been extended to allow for site clarifications."]
["Reason: Additional time provided for bidders to review technical clarifications and prepare compliant submissions."]
["Status: APPROVED - Addendum 3 issued 4 September 2026"]

{"sheet":"Addendum 2 - Cover","index":2,"n_rows":36,"n_cols":2,"rows_kept":36,"merged":[[15,0,15,1],[33,0,33,1],[34,0,34,1],[35,0,35,1]]}
["VALVE DATA PACKAGE - TENDER ADDENDUM"]
["TENDER E2979GXPOU"]
["Supply and Delivery of Various Valves and Valve Components for Peaking Power Stations"]
["ADDENDUM NO. 2"]
[]
["ADDENDUM DETAILS"]
["Issue Date:",{"$f":"\"28 August 2026\"","v":"28 August 2026"}]
["Revision:",2]
["Status:","ISSUED FOR TENDER"]
[]
["TENDER EXTENSION NOTICE"]
["Original Closing Date:","2026-08-20"]
["Extended Closing Date:","2026-09-17"]
[]
["SCOPE OF THIS ADDENDUM"]
["This addendum contains additional technical clarifications received from site end-users at various Peaking Power Stations in response to bidder queries."]
[]
["DOCUMENTS INCLUDED IN THIS ADDENDUM"]
["1. Technical Clarifications 2","18 items with site feedback (Published 28 August 2026)"]
[]
["SUMMARY OF CLARIFICATIONS"]
["Sites with clarifications:","Acacia PS, Drakensberg PSS, Ingula PSS, Port Rex PS, Vanderkloof PS"]
["Items clarified:",18]
["Information provided:","OEM/Brand, Part Numbers, Pressure Classes, Technical Specifications"]
[]
["REFERENCE DOCUMENTS (Original Tender Package)"]
["• Invitation to Tender (ITT) E2979GXPOU"]
["• Attachment 4 - Price List and Item Descriptions"]
["• Revised Price Schedule C2.2"]
["• Technical Clarifications (Revision 1)"]
["• Valve Data - All Sites"]
[]
["IMPORTANT NOTES"]
["All terms and conditions of the original Invitation to Tender remain applicable."]
["Bidders must submit technical datasheets for all items quoted."]
["Partial quotations are permitted - each line item evaluated independently."]

{"sheet":"Addendum 2 - Clarifications","index":3,"n_rows":55,"n_cols":7,"rows_kept":55,"merged":[[0,0,0,6],[1,0,1,6],[2,0,2,1],[2,2,2,3],[2,4,2,6],[22,0,22,6],[23,0,23,6],[24,0,24,6],[26,0,26,6],[27,0,27,6],[29,0,29,6],[30,0,30,6],[31,0,31,6],[32,0,37,2],[32,3,37,5],[39,0,44,2],[39,3,44,5],[46,0,51,2],[46,3,51,5],[53,0,53,6],[54,0,55,6]]}
["TENDER E2979GXPOU - OUTSTANDING INFORMATION FROM SITES - REVISION 2"]
["Where drawings unavailable, provide photographs of valve and nameplate."]
[{"$f":"\"Issue Date: 28 August 2026\"","v":"Issue Date: 28 August 2026"},null,"Revision: 2",null,"Status: ISSUED FOR TENDER"]
["No.","Site","Mat. No.","Description","Supplier Question","Eskom Response","Status Publish Date"]
[1,"Acacia PS",23900,"ASSEMBLY: AIR RELEASE VALVE FILTER; 42 IN","Process medium? Air filter or oil filter? OEM/Part Number?","Vent/air release valve used on Diesel filter vessel. During filling with diesel, it allows air to escape and closes/seals when diesel reaches the vent. Installed on top of vessel.",{"$f":"\"28 August 2026\"","v":"28 August 2026"}]
[2,"Drakensberg PSS",72044,"VALVE, GATE: 1/2 IN; WEDGE; BRS CAST; 1600 KPA; SABS 776","OEM/Brand/Part Number?","OEM/Brand: Hannifin/Festo.","28 August 2026"]
[3,"Drakensberg PSS",62540,"VALVE, SOLENOID: 220 V; P/N: S2155","Additional specifications? OEM/Brand?","OEM/Brand: Burkert South Africa.","28 August 2026"]
[4,"Port Rex PS",23886,"VALVE, BUTTERFLY: WAFER; 150 MM; FLANGE; STL; AIR OPERATED","Additional technical specifications?","Part Number: 1074195101NW. Same valve as Mat. No. 23887.","28 August 2026"]
[5,"Port Rex PS",23887,"VALVE, BUTTERFLY: WAFER; 150 MM; FLANGE; STL; AIR OPERATED","Additional technical specifications?","Part Number: 1074195101NW. Same valve as Mat. No. 23886.","28 August 2026"]
[6,"Vanderkloof PS",62654,"VALVE, GATE: 200 MM; SOLID WEDGE; FLANGE; CI; HANDWHEEL","Pressure class?","Pressure class: PN10 (10 bar / 1.0 MPa) or PN16 (16 bar / 1.6 MPa) - typical for 200 mm CI solid wedge flanged gate valve with handwheel.","28 August 2026"]
[7,"Drakensberg PSS",63152,"VALVE, GATE: 3/4 IN; SOLID WEDGE; FLANGE; BRASS; NEEDLE; BS 2060","Pressure class? Internal specification?","Pressure class: 150 lbs.","28 August 2026"]
[8,"Drakensberg PSS",72040,"VALVE, GATE: 3 IN; SOLID WEDGE; FLANGE; STEEL; 150 LB; HIRATA 2H27347","Quantities? Complete assemblies or spare parts? Duplicates?","Quantities: As Required (no specific quantity).","28 August 2026"]
[9,"Drakensberg PSS",72043,"VALVE, GLOBE: 10 MM; FNPT; STL FORGED; 150-800 LB; HIRATA 2N18553","Exact pressure class?","Exact pressure class: 150-800 lbs.","28 August 2026"]
[10,"Drakensberg PSS",72050,"VALVE, ANGLE: NEEDLE; 200 MM; 300 LB; FLANGE; STL CAST; HIRATA 2H18923","Direct handwheel or gear-operated?","Operation: Handwheel (direct).","28 August 2026"]
[11,"Drakensberg PSS",72056,"VALVE, GATE: 1/2 IN; SOLID WEDGE; FLANGE; STEEL; 150-800 LB; HIRATA 2M27352","Exact pressure class?","Exact pressure class: 150-800 lbs.","28 August 2026"]
[12,"Drakensberg PSS",72057,"VALVE, GATE: 100 MM; FLANGE; CS; 150 LB; HIRATA 2H27354","Complete technical specification (trim, stem, bonnet)?","Class 150, WCB carbon-steel body, flanged RF ends, bolted bonnet, rising stem (OS&Y), wedge gate.","28 August 2026"]
[13,"Drakensberg PSS",72058,"VALVE, GATE: 3/8 IN; SOLID WEDGE; FNPT; STEEL; 600 LB; HIRATA 2N27361","Quantities? Complete assemblies or spare parts? Duplicates?","Quantities: As Required (no specific quantity).","28 August 2026"]
[14,"Drakensberg PSS",72059,"VALVE, GLOBE: 1/2 IN; FNPT; STEEL; 150-200 LB; HIRATA 2S18669","Exact pressure rating?","Exact pressure rating: 150-200 lbs.","28 August 2026"]
[15,"Drakensberg PSS",72060,"VALVE, GLOBE: 10 MM; FNPT; SS FORGED; 150 LB; HIRATA 2S18670","Quantities? Complete assemblies or spare parts? Duplicates?","Quantities: As Required (no specific quantity).","28 August 2026"]
[16,"Drakensberg PSS",72062,"VALVE, GLOBE: 1/2 IN; FLANGE; STL FORGED; 150-800 LB; HIRATA 2M18627","Exact pressure class? Quantities? Duplicates?","Quantities: As Required (no specific quantity).","28 August 2026"]
[17,"Ingula PSS",721178,"VALVE, CHECK: TL34; 3 IN; DN80; 2 BAR; SERGI (FRANCE)","OEM requires serial numbers of TP systems.","OEM: SERGI (France). Type: TL34 Conservator Shutter Valve. Size: 3 IN / DN80. Rating: 2 BAR. Temp: -40 to 100°C. Body: ALSI7MG0.65T685HBS. Face-to-Face: 1.00 M. Max switching voltage: 250 VDC. Serial number for TP system not available.","28 August 2026"]
[18,"Drakensberg PSS",738160,"VALVE, NRV NON RETURN: 1/2 IN; 16 BAR; SS 316; SERGI FRANCE","OEM requires serial numbers of TP systems.","OEM: SERGI France. Type: NRV Non-Return Valve. Size: 1/2 IN. Rating: 16 BAR. Temp: -198 to 260°C. Body: SS 316. P/N: 111929400252002+00. Ref: FTTPDS48E 01. Serial number for TP system not available.","28 August 2026"]
["--- End of Clarifications ---"]
["ACACIA PS - Material 23900 (Air Release Valve Filter, 42 IN)"]
["Feedback: This is the vent/air release valve used on a Diesel filter vessel. During filling of the vessel with diesel, it allows air to escape and as soon as diesel reaches the vent it closes and seals. It is installed on top of the vessel."]
[]
["PORT REX PS - Materials 23886 & 23887 (Butterfly Valve, Wafer, 150 MM, Air Operated)"]
["Feedback: These 2 valves are the same valves. Part Number: 1074195101NW"]
[]
["PHOTOGRAPHS - Port Rex PS Butterfly Valves (Mat. 23886 & 23887) - P/N: 1074195101NW"]
["Photographs received from site (25 August 2026) - Port Rex PS Butterfly Valves (6 images in 2×3 grid):"]
["Images inserted below. Mat. 23886 / 23887 - P/N: 1074195101NW"]
[{"$error":"#VALUE!"},null,null,{"$error":"#VALUE!"}]
[]
[]
[]
[]
[]
[]
[{"$error":"#VALUE!"},null,null,{"$error":"#VALUE!"}]
[]
[]
[]
[]
[]
[]
[{"$error":"#VALUE!"},null,null,{"$error":"#VALUE!"}]
[]
[]
[]
[]
[]
[]
["NOTE TO BIDDERS:"]
["The above represents all available feedback from end-users as of Revision 2 (28 August 2026). Where information remains incomplete, bidders may indicate 'INSUFFICIENT DATA' per the bidder response options in the ITT. Bidders will not be penalised for omitting items where technical data is insufficient to provide a quotation. Partial quotations are permitted per ITT Clause 1.6."]

{"sheet":"Cover Sheet","index":4,"n_rows":48,"n_cols":2,"rows_kept":48,"merged":[[0,0,0,5],[1,0,1,5],[2,0,2,5],[3,0,3,5],[4,0,4,5]]}
["VALVE DATA PACKAGE - TENDER ADDENDUM"]
["TENDER E2979GXPOU"]
["Supply and Delivery of Various Valves and Valve Components for Peaking Power Stations"]
["Contract Period: Five (5) Years on an 'As and When Required' Basis"]
["TENDER EXTENSION: Closing date extended to 20 August 2026"]
["NOTICE TO BIDDERS"]
["This document contains valve data as received from site end-users at various Peaking Power Stations."]
["REFERENCE DOCUMENTS (Available from Eskom Tender Bulletin and National Treasury E-Tender Portal):"]
["• Invitation to Tender (ITT) E2979GXPOU"]
["• Attachment 4 - Price List and Item Descriptions"]
["• Revised Price Schedule C2.2"]
["• Technical Clarifications (included in this workbook - pre-clarification and post-clarification meeting queries)"]
["MANDATORY REQUIREMENT (Per ITT Section 3.13 - Functionality Criteria)"]
["Bidders must submit technical datasheets for all items quoted."]
["BIDDER RESPONSE OPTIONS (Per ITT):"]
["• QUOTED - Compliance with specifications (datasheet attached)"]
["• NOT QUOTING - Item not within bidder's product range"]
["• INSUFFICIENT DATA - Unable to quote; specify information required via official RFI process"]
["EVALUATION PROCESS (Per ITT Clauses 1.6, 2.22, 3.13, 3.15):"]
["• Partial quotations are permitted - each line item evaluated independently (Clause 1.6)"]
["• Alternative tenders are not allowed (Clause 2.22)"]
["• Minimum 70% functionality threshold applies (Clause 3.13)"]
["• Price evaluation per 90/10 (Clause 3.15)"]
["• Award may be to one or multiple suppliers on a line-item or category basis (Clause 1.6)"]
["CLARIFICATIONS:"]
["Bidders may submit Requests for Information (RFIs) through official procurement channels."]
["DATA SUMMARY:",{"$f":"COUNTA('Valve Data - All Sites'!A4:A999)","v":722}]
["Total Valve Records:",10]
["Number of Sites:"]
["INCLUDED SITES:"]
["1. Acacia Power Station"]
["2. Ankerlig Power Station"]
["3. Drakensberg Pumped Storage Scheme"]
["4. Gariep Hydro Power Station"]
["5. Gourikwa OCGT Power Station"]
["6. Ingula Pumped Storage Scheme"]
["7. Palmiet Pumped Storage Scheme"]
["8. Port Rex Gas Turbine Power Station"]
["9. Sere Wind Farm"]
["10. Vanderkloof Hydro Power Station"]
["TECHNICAL EVALUATION - INFORMATION REQUESTS:"]
["During the technical evaluation phase, Eskom reserves the right to request additional technical information, including but not limited to:"]
["• Detailed technical datasheets for quoted items"]
["• Clarification on technical specifications, materials, dimensions, or performance characteristics"]
["• Supporting documentation such as material certificates, test reports, or manufacturer declarations"]
["Bidders are required to respond to such requests within the timeframes specified by the evaluation committee."]
[]
["All terms and conditions of the Invitation to Tender and Eskom Standard Conditions of Tender remain applicable."]

{"sheet":"Technical Clarifications","index":5,"n_rows":17,"n_cols":7,"rows_kept":17,"merged":[[0,0,0,6],[1,0,1,6],[8,0,8,6],[9,0,9,6],[10,0,10,6],[11,0,11,6],[12,0,12,6],[13,0,13,6],[14,0,14,6],[15,0,15,6],[16,0,16,6]]}
["TENDER E2979GXPOU - TECHNICAL CLARIFICATIONS"]
["This addendum contains technical clarifications received pre-clarification meeting and post-clarification meeting. Refer to the 'Valve Data - All Sites' sheet or individual site sheets in this workbook and original tender documents."]
["Query No.","Date Received","Category","Query/Missing Information","Material Numbers Affected","Eskom Response","Status"]
["Q001","2026-06-02","General (Pre-Clarification)","Missing technical data identified: OEM/Manufacturer, Valve Type, Size, Body Material, Pressure Class/Rating, Trim Material, End Connection Details, Face-to-Face Dimensions, Flange Drilling/PCD, Operation Method, Process Medium, Operating Temperature, Design Pressure/Temperature. Request for customer to populate missing information from plant records, drawings, datasheets, OEM documentation or maintenance history.","All items","Refer to 'Valve Data - All Sites' sheet or individual site sheets in this workbook. Additional technical information has been populated where available from end-user records. Bidders may also refer to the Original Description in Attachment 4. Where information remains unavailable, bidders may submit RFIs through official procurement channels or indicate 'INSUFFICIENT DATA' per the bidder response options.","03.07.2026"]
["Q002","2026-06-18","Control Valves","Missing: Valve type, Flow characteristic, Cv/Kv coefficient, Pressure class, End connection standard, Body material grade, Trim material, Seat material, Leakage class, Actuator type, Signal type, Fail position","23899, 23909, 177857, 403617, 643634, 644441, 644442, 644443, 44480, 65784, 65807, 68767, 77249","Refer to 'Valve Data - All Sites' sheet or individual site sheets in this workbook and Attachment 4. Where OEM/Manufacturer is specified, products must meet OEM specifications. Where no OEM is specified, products meeting the stated technical specifications are acceptable. Technical datasheets are mandatory per ITT Section 3.13.","03.07.2026"]
["Q003","2026-06-18","Hydraulic Valves","Missing: Manufacturer, Mounting standard (ISO 4401/CETOP), Flow capacity (L/min), Pressure setting range, Pilot operation details, Coil voltage, Port size and thread type","623858, 623859, 701459, 644954","Refer to 'Valve Data - All Sites' sheet or individual site sheets in this workbook and Attachment 4. Where OEM/Manufacturer is specified, products must meet OEM specifications. Where no OEM is specified, products meeting the stated technical specifications are acceptable. Technical datasheets are mandatory per ITT Section 3.13.","03.07.2026"]
["Q004","2026-06-18","Globe Valves","Missing: Design Standard, Pressure Class, Body Material Grade, Trim Material, Seat Design, Bonnet Type, Stem Type, Flow Direction, Testing Requirements, Certification, Face-to-Face Standard","72060, 72062, 620183, 620407, 620408, 640478, 783503, 783422, 768522, 783424, 65808, 68910, 72018, 72038, 72039, 72041, 72043, 72045, 72059, 72054, 72061, 72063, 77228, 77229, 77231, 77243, 77236, 64665, 620181, 620186, 783504, 783648, 783651","Refer to 'Valve Data - All Sites' sheet or individual site sheets in this workbook and Attachment 4. Certification requirements: As specified in the Original Description or Valve Data sheets. Where specific certifications are stated, these must be provided. Technical datasheets are mandatory per ITT Section 3.13.","03.07.2026"]
["Q005","2026-06-24","General (OEM)","Request for clarity on OEMs required for the valves","All items","Refer to 'Valve Data - All Sites' sheet or individual site sheets in this workbook where OEM/Manufacturer information has been provided. Where OEM is specified, the product must meet OEM specifications. Where no OEM is specified, products meeting the stated technical specifications are acceptable. Per ITT Clause 2.22, alternative tenders are not allowed.","03.07.2026"]
["CERTIFICATION REQUIREMENTS:"]
["• Where certifications are specified in the Original Description or Valve Data sheets, these must be provided."]
["• Where not specified, industry standard certifications applicable to the valve type and application are required."]
["• Technical datasheets are mandatory per ITT Section 3.13."]
["OEM/MANUFACTURER REQUIREMENTS (Per ITT Clause 2.22):"]
["• Where OEM/Manufacturer is specified in the 'Valve Data - All Sites' sheet or individual site sheets: Products must meet OEM specifications."]
["• Where no OEM/Manufacturer is specified: Products meeting the stated technical specifications are acceptable."]
["• Alternative tenders are not allowed per ITT Clause 2.22."]
["TENDER EXTENSION NOTICE: The closing date for Tender E2979GXPOU has been extended to 20 August 2026."]

{"sheet":"Valve Data - All Sites","index":6,"n_rows":725,"n_cols":19,"rows_kept":725,"merged":[[0,0,0,18],[1,0,1,18]]}
["VALVE DATA PACKAGE - TENDER ADDENDUM E2979GXPOU - ALL SITES"]
["Datasheets required for all quoted items. Original tender documents available from Eskom Tender Bulletin and National Treasury E-Tender Portal."]
["Plant","Material","Original Description","OEM / Manufacturer","Valve Type","Size","Body Material","Class / Rating","Trim / Internals","End Connection","Face-to-Face","Drilling / PCD","Operation","Medium / Service","Medium Temperature","Material / Drawing / Reference No.","Actuator / Electrical Details","Seat / Softgoods","Certificates / Special Requirements"]
["Vanderkloof Hydro Power Station",62654,"VALVE, GATE: VALVE SIZE: 200 MM; TYPE: SOLID WEDGE; CONNECTION: FLANGE; BODY MATERIAL: CI; TRIM: BONNET CI; OPERATED: HANDWHEEL; STEM DESIGN: RISING OUTSIDE SCREW; STYLE: BOLTED BONNET; SUPPL P/N: Y1501-11","HITACHI","GATE; SOLID WEDGE","200 MM","CI",null,"BONNET CI; RISING OUTSIDE SCREW","FLANGE",null,null,"HANDWHEEL",null,null,"Y1501-11"]
["Vanderkloof Hydro Power Station",62793,"VALVE, SOLENOID: PIPE SIZE: 100 MM; STYLE: 2 WAY; POTENTIAL: 110/120 VAC; DESIGN RATING: 2.5 MPA; CONNECTION: FLANGE; BODY MATERIAL: STEEL; OPERATED: SOLENOID; ENCLOSURE RATING: IP 65 (EN 60529); MEDIUM: WATER; POWER: 220 VAC; CURRENT: 0.45 A; APPLICATION: GEN BEARING COOLER CW FLOW CONTROL; SPECIFICATION: PED; MANUF P/N: 8651000.9504.22050; REFERENCE NO: 27148735 & 27148736; SOLENOID VALVE INCLUDING A PISTON TYPE 2-WAY VALVE AND ELECTRICAL SOLENOID; DUTY CYCLE: 100% ED; VOLTAGE: FREQUENCY: 50HZ; VALVE MECHANICAL DETAILS: VALVE TYPE: 2/2 WAY PISTON VALVE; OPERATING PRESSURE: 0 - 25 BAR; RATED FLOW RATE: 125 M3/H = 34.7 L/S;VALVE MECHANICAL INTERFACE (FLANGE) DETAILS: FLANGE-TO-FLANGE FACE DIMENSION: 350MM; FLANGE STANDARD AND CLASS/TABLE: 100NB BS 4504 16/3;FLANGE OD = Ø220.0MM; RAISED FACE DIAMETER = Ø158.0MM; RAISED FACE HEIGHT = 3.0MM; NUMBER OF BOLTS = 8; BOLT HOLE DIAMETER = Ø18.0MM.","NORGREN","SOLENOID; 2/2 WAY PISTON VALVE","100 MM","STEEL","2.5 MPA",null,"FLANGE","350MM","BOLT HOLE DIAMETER = Ø18; 100NB BS 4504 16/3","SOLENOID","WATER; GEN BEARING COOLER CW FLOW CONTROL",null,"8651000.9504.22050; 27148735 & 27148736","110/120 VAC; 220 VAC; 0.45 A; IP 65 (EN 60529)"]
["Sere Wind Farm",621484,"VALVE, BUTTERFLY: TYPE: LUG WAFER; VALVE SIZE: 150 MM; DESIGN RATING: PN16; TEMPERATURE RATING: 0-120 DEG C; CONNECTION: LUG; BODY MATERIAL: DI; FACE TO FACE LENGTH: 59 MM; OPERATED: ACTUATOR; TRIM: RUBBER LINED; SOFTGOODS: SEAL; APPLICATION: TURBINE PROTECTION; GRADE: GGG40; SHAFT CONNECTION: DIA 14MM","Kennedy Valves","BUTTERFLY; LUG WAFER","150 MM","DI","PN16","RUBBER LINED","LUG; DIA 14MM","59 MM",null,"ACTUATOR","TURBINE PROTECTION","0-120 DEG C",null,null,"SEAL"]
["Port Rex Gas Turbine Power Station",23886,"VALVE, BUTTERFLY: TYPE: WAFER; VALVE SIZE: 150 MM; CONNECTION: FLANGE; BODY MATERIAL: STL; OPERATED: AIR; TRIM: DISC STL; ACTUATOR/ASSY,BLEED","Wood Group Pratt & Whitney Industrial Turbine Services, LLC (WGPW)","BUTTERFLY; WAFER","150 MM","STL",null,"DISC STL","FLANGE",null,null,"AIR"]
["Port Rex Gas Turbine Power Station",23887,"VALVE, BUTTERFLY: TYPE: WAFER; VALVE SIZE: 150 MM; CONNECTION: FLANGE; BODY MATERIAL: STL; OPERATED: AIR; TRIM: DISC STL; ACTUATOR AND VALVE ASSY; BLEED","Wood Group Pratt & Whitney Industrial Turbine Services, LLC (WGPW)","BUTTERFLY; WAFER","150 MM","STL",null,"DISC STL","FLANGE",null,null,"AIR"]
["Port Rex Gas Turbine Power Station",23899,"VALVE: TYPE: CONTROL; ASSY; AIR STARTER","Wood Group Pratt & Whitney Industrial Turbine Services, LLC (WGPW)","CONTROL"]
["Port Rex Gas Turbine Power Station",23905,"VALVE, SOLENOID: PIPE SIZE: 25 MM; STYLE: 2 WAY; POTENTIAL: 110 VAC; 120 VDC; DESIGN RATING: 115/225/300 KPA; CONNECTION: FNPT; BODY MATERIAL: BRASS; OPERATED: AIR; ENCLOSURE RATING: IP67; MEDIUM: AIR/GAS/WATER; POWER: 20 W; ORIFICE SIZE: 25 MM; FREQUENCY 50/60 HZ, FOR USE ON COMPRESSOR",null,"SOLENOID","25 MM","BRASS","115/225/300 KPA",null,"FNPT",null,null,"AIR","AIR/GAS/WATER; COMPRESSOR",null,null,"110 VAC; 20 W; IP67"]
["Port Rex Gas Turbine Power Station",62790,"VALVE, SOLENOID: PIPE SIZE: 8 MM; STYLE: 2 WAY; POTENTIAL: 120 VAC; DESIGN RATING: 150 LB; CONNECTION: FNPT; BODY MATERIAL: STEEL; MEDIUM: AIR/LIQUID; POWER: 10 W; ORIFICE SIZE: 1/16 X 3/64 IN; 60 HZ; GENERAL PURPOSE ENCLOSURE",null,"SOLENOID","8 MM; 1/16 X 3/64 IN","STEEL","150 LB",null,"FNPT",{"$nulls":3},"AIR/LIQUID",null,null,"120 VAC; 10 W"]
["Port Rex Gas Turbine Power Station",74427,"SEAL, RING: TYPE: VALVE END; INSIDE DIAMETER: 58 MM; OUTSIDE DIAMETER: 62 MM; THICKNESS: 3 MM; MATERIAL: TEFLON; APPLICATION: VALVE; REFERENCE NO: 20117-16",null,"VALVE END",null,"TEFLON",{"$nulls":6},"VALVE",null,"20117-16"]
["Port Rex Gas Turbine Power Station",256828,"VALVE: TYPE: LIQUID FUEL METERING; VALVE SIZE: 193.5 MM2; DESIGN RATING: 345 KPA; TEMPERATURE RATING: -28 TO +103 DEG C; CONNECTION: BASE; OPERATED: ELECTRICAL; BODY MATERIAL: METAL; MANUF P/N: LQ25, 9907-361; SUPPL P/N: LQ25T","Wood Group Pratt & Whitney Industrial Turbine Services, LLC (WGPW)","LIQUID FUEL METERING","193.5 MM2","METAL","345 KPA",null,"BASE",null,null,"ELECTRICAL",null,"-28 TO +103 DEG C","LQ25, 9907-361; LQ25T"]
["Port Rex Gas Turbine Power Station",589427,"VALVE, RELIEF: VALVE SIZE: 3/4 IN; SET PRESSURE: 420 KPA; TEMPERATURE RATING: 70 DEG C; CONNECTION: THD 1/2 IN; BODY MATERIAL: BRASS; TRIM: PLASTIC BONNET/ADJUSTABLE SCREW; FACE TO FACE LENGTH: 65 MM; OPERATED: PRESSURE 0-460 KPA; DESIGN RATING: 40 BAR; PRESSURE RANGE: 0-40 BAR; MANUF P/N: D22-1/2A",null,"RELIEF","3/4 IN","BRASS","40 BAR; 0-40 BAR; 420 KPA","PLASTIC BONNET/ADJUSTABLE SCREW","THD 1/2 IN","65 MM",null,"PRESSURE 0-460 KPA",null,"70 DEG C","D22-1/2A"]
["Palmiet Pumped Storage Scheme",43039,"HEAD, CYLINDER: TYPE: 1ST STG VALVE; SUPPL P/N: 4656; ITEM 23 POS 230, SIZE 128MM X 128 MM X 20 MM;USED ON THE SULZER BURCKHART COMPRESSOR TYPE C4N2F","C4N2F","1ST STG VALVE",{"$nulls":8},"THE SULZER BURCKHART COMPRESSOR TYPE C4N2F",null,4656]
["Palmiet Pumped Storage Scheme",62308,"VALVE, RELIEF: VALVE SIZE: 24 X 12 MM; SET PRESSURE: 14.5 KGF/CM; CONNECTION: NPT X FNPT; BODY MATERIAL: BRASS; REFERENCE NO: M096-84176222/23P10; SAFETY; POP; TYPE RCX-SO; SEAT DIA. 12MM","RCX-SO","RELIEF","24 X 12 MM","BRASS","14.5 KGF/CM",null,"NPT X FNPT",{"$nulls":5},"M096-84176222/23P10",null,"M"]
["Palmiet Pumped Storage Scheme",62309,"VALVE, SOLENOID: PIPE SIZE: 1/4 IN; STYLE: 3 WAY; POTENTIAL: 220 VDC; DESIGN RATING: 35 KGF/CM; CONNECTION: FNPT; BODY MATERIAL: BRASS; MEDIUM: AIR/GAS/OIL/WATER; POWER: 9.7 W; ORIFICE SIZE: 3/64 IN; DRAWING NO: M096-8417222/23P8 REV 1; CAT NO: T8262D19; REFERENCE NO: 364202; 8321A2; GENERAL PURPOSE ENCLOSURE","ASCO","SOLENOID","1/4 IN; 3/64 IN","BRASS","35 KGF/CM",null,"FNPT",{"$nulls":3},"AIR/GAS/OIL/WATER",null,"364202; M096-8417222/23P8 REV 1; T8262D19","220 VDC; 9.7 W"]
["Palmiet Pumped Storage Scheme",62311,"VALVE, SOLENOID: PIPE SIZE: 3/8 IN; STYLE: 2 WAY; POTENTIAL: 220 VDC; DESIGN RATING: 0.7/14 KGF/CM; CONNECTION: FNPT; BODY MATERIAL: BRASS; MEDIUM: AIR/GAS/OIL/WATER; POWER: 9.7 W; ORIFICE SIZE: 9/32 IN; REFERENCE NO: 364201; 8263D19; GENERAL PURPOSE ENCLOSURE","ASCO","SOLENOID","3/8 IN; 9/32 IN","BRASS","0.7/14 KGF/CM",null,"FNPT",{"$nulls":3},"AIR/GAS/OIL/WATER",null,364201,"220 VDC; 9.7 W"]
["Palmiet Pumped Storage Scheme",62312,"VALVE, SOLENOID: PIPE SIZE: 10 MM; STYLE: 4/2 WAY; POTENTIAL: 250 VAC; DESIGN RATING: 315 BAR; CONNECTION: COMPRESSION; BODY MATERIAL: STEEL; OPERATED: DC SOLENOID; ENCLOSURE RATING: IP54; MEDIUM: AIR/LIQUID; POWER: 36 W; MANUF P/N: S10G51G0230615MV; CAT NO: 52051.9000; HERION DIRECTIONAL CONTROL VALVE - PRESSURE TEST CERTIFICATES TO BE SUPPLIED ON DELIVERY","Herion","SOLENOID","10 MM","STEEL","315 BAR",null,"COMPRESSION",null,null,"DC SOLENOID","AIR/LIQUID",null,"S10G51G0230615MV; 52051.9000","250 VAC; 36 W; IP54",null,"PRESSURE TEST CERTIFICATES TO BE SUPPLIED ON DELIVERY; CERTIFICATES TO BE SUPPLIED ON DELIVERY"]
["Palmiet Pumped Storage Scheme",177857,"VALVE: TYPE: CONTROL; VALVE SIZE: 38 MM; CONNECTION: FLANGE; OPERATED: AIR; BODY MATERIAL: CS; STYLE: BOLTED BONNET; TRIM: DISC STL","Fisher","CONTROL","38 MM","CS",null,"DISC STL","FLANGE",null,null,"AIR"]
["Palmiet Pumped Storage Scheme",664392,"VALVE: TYPE: PLUG; VALVE SIZE: DN 150; DESIGN RATING: PN64; TEMPERATURE RATING: 0-100 DEG C; CONNECTION: FLANGE DN150/PN64; OPERATED: HYDRAULIC; BODY MATERIAL: CS; SUPPL P/N: 2612; VOITH RUNNER RELIEF VALVE; ORDER NUMBER: 5/5044; TYPE: 2.41-48660 PRESSURE TEST CERTIFICATES TO BE SUPPLIED WITH VALVE; VALVE DRAWING WITH BILL OF MATERIALS/PARTS LIST TO BE SUPPLIED","Voith","PLUG; 2.41-48660 PRESSURE TEST CERTIFICATES TO BE SUPPLIED WITH VALVE","DN 150","CS","PN64",null,"FLANGE DN150/PN64",null,null,"HYDRAULIC",null,"0-100 DEG C",2612,null,null,"PRESSURE TEST CERTIFICATES TO BE SUPPLIED WITH VALVE; CERTIFICATES TO BE SUPPLIED WITH VALVE"]
["Palmiet Pumped Storage Scheme",688401,"VALVE, RELIEF: VALVE SIZE: 100 X 125 MM; SET PRESSURE: 25-2400 KPA G; TEMPERATURE RATING: -4 TO -230 DEG C; CONNECTION: FLANGE; BODY MATERIAL: CS; TRIM: DISC ST/ST; FACE TO FACE LENGTH: 187/165 MM; OPERATED: SPRING; ORIFICE SIZE: SQ 2027 MM; SPECIFICATION: BS 6759-3:1984; APPLICATION: BFPT LUB OIL BYPASS PRESSURE; SOFTGOODS: GASKET INORGANIC FIBRE WITH NITRILE BINDER; DESIGN RATING: 2.4 MPA; REFERENCE NO: 693; SC81S503 & SC71S09; INLET FACE TO OUTLET CENTRE 187 MM; OUTLET FACE TO INLET CENTRE 16 5 MM; CAST STEEL SINGLE SPRING HIGH LIFT SAFETY RELIEF VALVE; INLET FLANGE DN 100 BS10-H; OUTLET FLANGE DN125 BS10-F; SPRING OPERATED TO OPEN WHEN SET SPRING TENSION IS OVERCOME BY SYSTEM PRESSURE; SEAT RING ST/ST; SPRING STEEL; ALL OTHER DIMENSIONS TO BS 6759-3:1984; VALVE TO BE SUPPLIED WITH A SET PRESSURE CERTIFICATE; FLANGES TO BE COVERED OR PLUGGED TO PREVENT FOREIGN MATERIAL FROM ENTERING, AND PROTECTED FROM THE ELEMENTS WITH A SUITABLE CORROSION INHIBITOR; A TECHNICAL EVALUATION NEEDS TO BE DONE PRIOR TO ORDER PLACEMENT; THE FOLLOWING DOCUMENTS ARE REQUIRED FOR THE TECHNICAL EVALUATION (1) GENERAL VALVE ASSEMBLY DRAWING (2) VALVE BROCHURE/INFORMATION; SIGNED ASSEMBLY DRAWING BY THE SUPPLIER WILL SERVE AS PROOF FOR THE CORRECT ITEM TO BE SUPPLIED; NO QUALITY CHECK WILL BE DONE WITHOUT A TECHNICAL EVALUATION BEING DONE DURING THE TENDERING STAGE; FOR VALVES THAT ARE TO BE REFURBISHED, A REFURBISHED SOW MUST BE SUBMITTED BY TURBINE ENGINEERING; THIS SOW MUST BE ISSUED WITH THE TENDERS; NO REPAIRS WILL BE PERMITTED OR ACCEPTED WITHOUT THE ENGINEERING SOW BEING SUPPLIED AND ADHERED TO","LESER","RELIEF","100 X 125 MM; SQ 2027 MM","CS","2.4 MPA; 25-2400 KPA G","DISC ST/ST","FLANGE","187/165 MM",null,"SPRING","BFPT LUB OIL BYPASS PRESSURE","-4 TO -230 DEG C",693,null,"GASKET INORGANIC FIBRE WITH NITRILE BINDER; T","CERTIFICATE; TECHNICAL EVALUATION NEEDS TO BE DONE PRIOR TO ORDER PLACEMENT; TECHNICAL EVALUATION (1) GENERAL VALVE ASSEMBLY DRAWING (2) VALVE BROCHURE/INFORMATION; TECHNICAL EVALUATION BEING DONE DURING THE TENDERING STAGE"]
["Palmiet Pumped Storage Scheme",714976,"VALVE, PLUG: VALVE SIZE: 80; DESIGN RATING: PN40; TEMPERATURE RATING: -10 TO 100 CELSIUS; CONNECTION: THREADED CONNECTION (G1/2); BODY MATERIAL: CARBON STEEL; FACE TO FACE LENGTH: 155 MM; OPERATED: HYDRAULIC; SOFTGOODS: O-RING RUBBER 85X3 / O-RING RUBBER 102X3 / MANTEL-RING TFMA 90X88X7.3 / NUT-RINGB12X24X10 / SCRAPER-RING B12X22; CONFIGURATION: FLANGE; APPLICATION: COMPRESSED AIR; TYPE: BLOWDOWN; MANUF P/N: 2.49-581","SchuF Group","PLUG; BLOWDOWN",80,"CARBON STEEL","PN40",null,"THREADED CONNECTION (G1/2)","155 MM",null,"HYDRAULIC","COMPRESSED AIR","-10 TO 100 CELSIUS","2.49-581",null,"O-RING RUBBER 85X3 / O-RING RUBBER 102X3 / MANTEL-RING TFMA 90X88X7.3 / NUT-RINGB12X24X10 / SCRAPER-RING B12X22"]
["Palmiet Pumped Storage Scheme",728675,"VALVE, RELIEF: VALVE SIZE: 1 IN; SET PRESSURE: 64 BAR; TEMPERATURE RATING: -30 TO 100 DEG C; CONNECTION: G1 IN; BODY MATERIAL: FREE CUTTING STEEL; TRIM: FREE CUTTING STEEL; FACE TO FACE LENGTH: 115 MM; OPERATED: PILOT; APPLICATION: HYDRAULIC PUMP; STYLE: SPOOL TYPE; SOFTGOODS: NBR O-RINGS; DESIGN RATING: 125 BAR; PRESSURE RANGE: 5 -125 BAR; MANUF P/N: DB16P; MODEL NO: DB16P-01-C-N-190V","Yuken","RELIEF","1 IN","FREE CUTTING STEEL","125 BAR; 5 -125 BAR; 64 BAR","FREE CUTTING STEEL","G1 IN","115 MM",null,"PILOT","HYDRAULIC PUMP","-30 TO 100 DEG C","DB16P; DB16P-01-C-N-190V",null,"NBR O-RINGS"]
["Palmiet Pumped Storage Scheme",731743,"VALVE, CHECK: TYPE: SWING DISK NRV; VALVE SIZE: 3 IN; DESIGN RATING: PN 16; TEMPERATURE RATING: 0 TO 100 DEG C; CONNECTION: FLANGED; BODY MATERIAL: ASTM 216; FACE TO FACE LENGTH: 66 MM; OPERATED: SPRING ACTUATED; STYLE: WAFER TYPE SWING CHECK; SPECIFICATION: FM,UL,CUL APPROVED; MANUF P/N: V03312; PRESSURE TEST AND MATERIAL TEST CERTIFICATES TO BE SUPPLIED UPON DELIVERY OF THE VALVES.","SWING","CHECK; SWING DISK NRV","3 IN","ASTM 216","PN 16",null,"FLANGED","66 MM",null,"SPRING ACTUATED",null,"0 TO 100 DEG C","V03312",null,null,"PRESSURE TEST AND MATERIAL TEST CERTIFICATES TO BE SUPPLIED UPON DELIVERY OF THE VALVES; MATERIAL TEST CERTIFICATES TO BE SUPPLIED UPON DELIVERY OF THE VALVES; CERTIFICATES TO BE SUPPLIED UPON DELIVERY OF THE VALVES"]
["Palmiet Pumped Storage Scheme",731847,"VALVE, RELIEF: VALVE SIZE: G 1/4 IN; SET PRESSURE: 11 BAR; TEMPERATURE RATING: -20 TO 200 DEG C; CONNECTION: THREADED; BODY MATERIAL: BRASS; TRIM: BRASS - STAINLESS STEEL; FACE TO FACE LENGTH: 65 MM; OPERATED: SPRING LOADED - MECHANICALLY; ORIFICE SIZE: 38.47 MM2; SPECIFICATION: ASME VIII DIV. 1; APPLICATION: COMPRESSED AIR; STYLE: FREE DISCHARGE - D7; SOFTGOODS: N.B.R.(STD) -10 / + 100 °C; DESIGN RATING: PN60; PRESSURE RANGE: 8 - 12 BAR; MANUF P/N: D7CW614N; SAFETY VALVE TO BE SET AT 11 BAR (COLD SET PRESSURE). SAFETY VALVE TO BE TAGGED AND LED SEALED. INFORMATION ON TAG SHOULD CONTAIN:VALVE SERIAL NUMBER, SET PRESSURE, TEST DATE AND DUE DATE. DUE DATE SHOULD BE 3 YEARS FROM TEST DATE. VALVE. TEST REPORT TO BE SUPPLIED ALONG WITH VALVE.TEST REPORT TO DETAIL TO CORRESPOND WITH VALVE INFO","Nuova General Instruments S.r.l.","RELIEF","G 1/4 IN; 38.47 MM2","BRASS","PN60; 8 - 12 BAR; 11 BAR","BRASS - STAINLESS STEEL","THREADED","65 MM",null,"SPRING LOADED - MECHANICALLY","COMPRESSED AIR","-20 TO 200 DEG C","D7CW614N",null,"N.B.R.(STD) -10 / + 100 °C","TEST REPORT TO BE SUPPLIED ALONG WITH VALVE; TEST REPORT TO DETAIL TO CORRESPOND WITH VALVE INFO"]
["Palmiet Pumped Storage Scheme",767444,"VALVE: TYPE: PRESSURE RELIEF; VALVE SIZE: 1/4 IN; DESIGN RATING: 0.3-10 BAR; TEMPERATURE RATING: -34 TO 65 DEG C; CONNECTION: G1/4 IN; OPERATED: 10BAR; BODY MATERIAL: ZINC ALLOY; MANUF P/N: V07-200NGMG; V07; NORGREN, MINIATURE PORTED","Norgren","PRESSURE RELIEF","1/4 IN","ZINC ALLOY","0.3-10 BAR",null,"G1/4 IN",null,null,"10BAR",null,"-34 TO 65 DEG C","V07-200NGMG"]
["Palmiet Pumped Storage Scheme",28911,"BELT: TYPE: VALVE; FIG NO: 2396C.S. SA1253 B77; REFERENCE NO: 44411-006B; FOR 3 INCH HOPKINSON VALVE; USED FOR SOOTBLOWER REHEAT SECTION; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","No further information available","VALVE",{"$nulls":10},"44411-006B; 2396C.S. SA1253 B77"]
["Palmiet Pumped Storage Scheme",68400,"VALVE, CHECK: VALVE SIZE: 20 MM; DESIGN RATING: 20 BAR; TEMPERATURE RATING: 9 BAR AT 180 DEG C; CONNECTION: THD FEMALE; BODY MATERIAL: BRZ; STYLE: THD CAP; TRIM: DISC BRZ; MODEL NO: SS3501/M; REFERENCE NO: ES701; TYPE LIFT; IN LINE; CKI; FOR USE ON BOILER; MATERIAL AND TEST CERTIFICATES, TO DIN 50049/3.1B, ARE TO BE SUPPLIED ON DELIVERY","LIFT","CHECK","20 MM","BRZ","20 BAR","DISC BRZ","THD FEMALE",{"$nulls":3},"BOILER","9 BAR AT 180 DEG C","ES701; SS3501/M",null,null,"CERTIFICATES, TO DIN 50049/3"]
["Palmiet Pumped Storage Scheme",68955,"VALVE, CHECK: TYPE: SWING; VALVE SIZE: 280 MM; TEMPERATURE RATING: 200 DEG C; CONNECTION: BW; STYLE: BOLTED CAP; TRIM: DISC/SEAT 13CRS; GRADE: WCB; WEIGHT ASSISTED; BODY 37.5BAR; SEAT 25BAR","NEWAY","CHECK; SWING","280 MM",null,null,"DISC/SEAT 13CRS","BW",{"$nulls":4},"200 DEG C",null,null,"S; R"]
["Palmiet Pumped Storage Scheme",515330,"MASK: TYPE: DUST; DIMENSIONS: 207 MM; PROTECTION FOR WHICH DESIGNED: DUST; SPECIAL FEATURES: WITH VALVE; SUPPL P/N: FFP2; PPE","No further information available","DUST",{"$nulls":10},"FFP2"]
["Palmiet Pumped Storage Scheme",751707,"VALVE, GATE: VALVE SIZE: DN150 MM; TYPE: WEDGE; DESIGN PRESSURE: 16 BAR; DESIGN TEMPERATURE: +/- 80 DEG C; CONNECTION: FLANGE; FACE TO FACE LENGTH: 210 MM; BODY MATERIAL: CAST IRON; TRIM: WEDGE; OPERATED: HANDWHEEL; STEM DESIGN: RISING SPINDLE; TEMPERATURE RATING: +/- 80 DEG C; APPLICATION: COOLING TOWERS ISOLATION; DESIGN RATING: 16 BAR; OPERATED: HANDWHEEL RISING SPINDLE; DESIGN RATING: 16 BAR; DRILING: SANS1123 – TABLE 600","AVK","GATE; WEDGE","DN150 MM","CAST IRON","16 BAR","WEDGE; RISING SPINDLE","FLANGE","210 MM","SANS1123 – TABLE 600","HANDWHEEL; HANDWHEEL RISING SPINDLE","COOLING TOWERS ISOLATION","+/- 80 DEG C"]
["Palmiet Pumped Storage Scheme",751861,"VALVE, CHECK: TYPE: WAFER; VALVE SIZE: 400 MM; DESIGN RATING: 1600 KPA; TEMPERATURE RATING: 0 TO 100 DEG C; CONNECTION: FLANGE; BODY MATERIAL: CF8M; FACE TO FACE LENGTH: 108 MM; OPERATED: SPRING ACTUATED; STYLE: WAFER; TRIM: CF8M; SOFTGOODS: NITRILE; OEM P/N: 16DMZ; MODEL NO: 16DMZ; FIG NO: 16DMZ, SERIAL NO:821186, PRESSURE TEST AND MATERIAL TEST CERTIFICATES TO BE SUPPLIED WITH VALVES.","NEWAY","CHECK; WAFER","400 MM","CF8M","1600 KPA","CF8M","FLANGE","108 MM",null,"SPRING ACTUATED",null,"0 TO 100 DEG C","16DMZ; 16DMZ, SERIAL NO:821186, PRESSURE TEST AND MATERIAL TEST CERTIFICATES TO BE SUPPLIED WITH VALVES",null,"NITRILE","PRESSURE TEST AND MATERIAL TEST CERTIFICATES TO BE SUPPLIED WITH VALVES; MATERIAL TEST CERTIFICATES TO BE SUPPLIED WITH VALVES; CERTIFICATES TO BE SUPPLIED WITH VALVES"]
["Palmiet Pumped Storage Scheme",762729,"VALVE, RELIEF: VALVE SIZE: 172 X 90 MM; SET PRESSURE: 8 PSI; TEMPERATURE RATING: -30 TO -120 DEG C; CONNECTION: FLANGE; BODY MATERIAL: WEATHERPROOF AND TRANSFORMER OIL RESISTANT ALUMINIUM; TRIM: SPRING STEEL EN 10270-1; OPERATED: SPRING; SPECIFICATION: IEC 60947-5-1 AC-15 / DC-13; APPLICATION: PALMIET GEN TRANSFORMER; STYLE: SIGNAL PIN INDICATOR; SOFTGOODS: MOUNTING GASKET 200 X 178.5 X 4.25 MM","MESSKO","RELIEF","172 X 90 MM","WEATHERPROOF AND TRANSFORMER OIL RESISTANT ALUMINIUM","8 PSI","SPRING STEEL EN 10270-1","FLANGE",null,null,"SPRING","PALMIET GEN TRANSFORMER","-30 TO -120 DEG C",null,null,"MOUNTING GASKET 200 X 178.5 X 4.25 MM"]
["Palmiet Pumped Storage Scheme",778355,"PROTECTOR: TYPE: SHUTTER VALVE; DIMENSIONS: 80 MM; MATERIAL: ALUMINIUM; MANUF P/N: 1RDR100800; POWER SUPPLY 220V AC OR DC, BREAKING CAPACITY 2A, RATED CURRENT 0.5A FOR 10.000 MANOEUVERS","COMEM","SHUTTER VALVE",null,"ALUMINIUM",{"$nulls":8},"1RDR100800"]
["Palmiet Pumped Storage Scheme",717459,"VALVE: TYPE: HYDRAULIC; VALVE SIZE: 0.5 MM; DESIGN RATING: 65 BAR; TEMPERATURE RATING: -10 TO 100 BAR; FACE TO FACE LENGTH: 286 MM; CONNECTION: BSP 1/4 IN / 1/2 BSP IN; OPERATED: HYDRAULIC; BODY MATERIAL: CARBON STEEL-UPPER AND MIDDLE BLOCK BRASS -; STYLE: UPPER BLOCK COMPRESSION SPRING - MIDDLE BLOCK HYDRAULIC -LOWER BLOCK WATER; TRIM: COMPRESSION SPRING 35X45X100 - WIRE 5MM - COILS 8; SOFTGOODS: 8X2NBR70 ORINGS -32X3NBR ORINGS -20X3BNR70 ORINGS; SPECIAL FEATURES: HYDRAULIC TELL TALE HOLES,PILOTED WITH WATER; MANUF P/N: 3/5010 2.41-32489; SQUARE TYPE O RING,TAPPERED BOTTOM THICKNESS 4MM PAPER 5.3 - 6.3 MM ID 11 MM OD 21 MM TAPERED BOTTOM 21.6 PAPERED TOP 11 MM, MANTEL RING TFMI 16X18X3/19X2.5 MM O-RING HYDRAULIC MIDDLE SECTION M10 MOUTING HOLES","No further information available","HYDRAULIC","0.5 MM","CARBON STEEL-UPPER AND MIDDLE BLOCK BRASS -","65 BAR","COMPRESSION SPRING 35X45X100 - WIRE 5MM - COILS 8","BSP 1/4 IN / 1/2 BSP IN","286 MM",null,"HYDRAULIC",null,"-10 TO 100 BAR","3/5010 2.41-32489",null,"8X2NBR70 ORINGS -32X3NBR ORINGS -20X3BNR70 ORINGS"]
["Palmiet Pumped Storage Scheme",41764,"VALVE: TYPE: UNLOADING; FOR CONDENSATE B/DOWN","No further information available","UNLOADING"]
["Palmiet Pumped Storage Scheme",41832,"VALVE: TYPE: COMPRESSOR; VALVE SIZE: 280 MM; OPERATED: PRESSURE; BODY MATERIAL: STL; TRIM: DISC SS; 1ST STAGE CONCENTRIC","No further information available","COMPRESSOR","280 MM","STL",null,"DISC SS",{"$nulls":3},"PRESSURE"]
["Palmiet Pumped Storage Scheme",41833,"VALVE: TYPE: COMPRESSOR; VALVE SIZE: 175 MM; OPERATED: PRESSURE; BODY MATERIAL: STL; TRIM: DISC SS; 2ND STAGE CONCENTRIC","No further information available","COMPRESSOR","175 MM","STL",null,"DISC SS",{"$nulls":3},"PRESSURE"]
["Palmiet Pumped Storage Scheme",41834,"VALVE: TYPE: COMPRESSOR; VALVE SIZE: 95 MM; OPERATED: PRESSURE; BODY MATERIAL: STL; TRIM: DISC SS; 3RD STAGE CONCENTRIC","No further information available","COMPRESSOR","95 MM","STL",null,"DISC SS",{"$nulls":3},"PRESSURE"]
["Palmiet Pumped Storage Scheme",50087,"VALVE, SOLENOID: PIPE SIZE: 15 MM; STYLE: 2 WAY; CONNECTION: FNPT; BODY MATERIAL: STEEL; MEDIUM: OIL; SUPPL P/N: 2VA2/43A-002/1 T6; DISTRIBUTION BLOCK","No further information available","SOLENOID","15 MM","STEEL",null,null,"FNPT",{"$nulls":3},"OIL",null,"2VA2/43A-002/1 T6"]
["Palmiet Pumped Storage Scheme",50088,"VALVE, SOLENOID: PIPE SIZE: 12 MM; STYLE: 4 WAY; CONNECTION: FNPT; BODY MATERIAL: STEEL; MEDIUM: OIL; SUPPL P/N: ZVA 2/22A-002/1 T6; DISTRIBUTION BLOCK 1 WAY","No further information available","SOLENOID","12 MM","STEEL",null,null,"FNPT",{"$nulls":3},"OIL",null,"ZVA 2/22A-002/1 T6"]
["Palmiet Pumped Storage Scheme",50089,"VALVE, SOLENOID: PIPE SIZE: 12 MM; STYLE: 3 WAY; CONNECTION: FNPT; BODY MATERIAL: STEEL; MEDIUM: OIL; SUPPL P/N: ZA2-66A-002/1 T6; DISTRIBUTION BLOCK","No further information available","SOLENOID","12 MM","STEEL",null,null,"FNPT",{"$nulls":3},"OIL",null,"ZA2-66A-002/1 T6"]
["Palmiet Pumped Storage Scheme",50090,"VALVE, SOLENOID: PIPE SIZE: 15 MM; STYLE: 2 WAY; CONNECTION: FNPT; BODY MATERIAL: STEEL; MEDIUM: OIL; SUPPL P/N: ZVA2-44A-002-1 T6; DISTRIBUTION BLOCK","No further information available","SOLENOID","15 MM","STEEL",null,null,"FNPT",{"$nulls":3},"OIL",null,"ZVA2-44A-002-1 T6"]
["Palmiet Pumped Storage Scheme",50092,"VALVE, SOLENOID: PIPE SIZE: 12 MM; STYLE: 4 WAY; CONNECTION: FNPT; BODY MATERIAL: STEEL; MEDIUM: OIL; SUPPL P/N: ZVA2-88A-002-1 T6; DISTRIBUTION BLOCK","No further information available","SOLENOID","12 MM","STEEL",null,null,"FNPT",{"$nulls":3},"OIL",null,"ZVA2-88A-002-1 T6"]
["Palmiet Pumped Storage Scheme",69346,"VALVE, RELIEF: VALVE SIZE: 30 X 15 MM; SET PRESSURE: 64 BAR; CONNECTION: NPT X FNPT; BODY MATERIAL: STL; TRIM: DISC SS; SPRING STL; OPERATED: PRESSURE, SPRING; FULL STROKE SPRING TYPE SAFETY; GEBR LESER TYPE 561; D/G 0.8; BEST NUMBER: 615875/5003","SAFETY; Leser","RELIEF","30 X 15 MM","STL","64 BAR","DISC SS","NPT X FNPT",null,null,"PRESSURE, SPRING"]
["Palmiet Pumped Storage Scheme",69359,"VALVE, PLUG: VALVE SIZE: 15 MM; CONNECTION: FNPT; BODY MATERIAL: BRASS; OPERATED: HANDWHEEL; STYLE: THD BONNET; TRIM: BONNET/PLUG BRS; TYPE: SHUT OFF; DRAWING NO: M096-84176222/23P9 REV 1; REFERENCE NO: NBV1003GX; PACKLESS; RIGHT - LEFT OPEN INDICATION; 3/8 INCH; MP 30KG/CM","DATA NOT AVAILABLE","PLUG; SHUT OFF","15 MM","BRASS",null,"BONNET/PLUG BRS","FNPT",null,null,"HANDWHEEL",null,null,"NBV1003GX; M096-84176222/23P9 REV 1"]
["Palmiet Pumped Storage Scheme",142398,"CLUTCH: TYPE: SOLENOID VALVE; BORE: 19 MM; DRAWING NO: HATM 302903 P001 REV 1; 110 VOLT; SIZE OD 85.7 X WD 38.4MM; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","No further information available","SOLENOID VALVE",{"$nulls":10},"HATM 302903 P001 REV 1"]
["Palmiet Pumped Storage Scheme",655128,"VALVE, BUTTERFLY: TYPE: STRAINER; VALVE SIZE: DN50; DESIGN RATING: 16 BAR; TEMPERATURE RATING: -10 TO 110 DEG C; CONNECTION: MALE COUPLING; BODY MATERIAL: CI; FACE TO FACE LENGTH: 45 MM; OPERATED: ACTUATOR; TRIM: DISC SS; SHAFT SS;BODY SEAT EPDM; SOFTGOODS: RUBBER; SUPPL P/N: IBF3SS","AVK","BUTTERFLY; STRAINER","DN50","CI","16 BAR","DISC SS","MALE COUPLING","45 MM",null,"ACTUATOR",null,"-10 TO 110 DEG C","IBF3SS",null,"RUBBER; M"]
["Palmiet Pumped Storage Scheme",725188,"VALVE: TYPE: AIR VENT; VALVE SIZE: 3/4 X 3/8 IN; DESIGN RATING: 16 BAR; TEMPERATURE RATING: 120 DEG C; FACE TO FACE LENGTH: 1.5 MM; CONNECTION: INLET 3/4 NPT FEMALE X EXHAUSE 3/8 NPP FEMALE STRAIGHT; OPERATED: AIR; BODY MATERIAL: BRASS,INTERNAL: STAINLESS, SEAL :PEAK,NBR FKM; STYLE: POT SHAPED; TRIM: FLOAT TYPE AUTOMATIC; SOFTGOODS: O RING RUBBER; SPECIAL FEATURES: CALEFFI; MANUF P/N: 501500; ART 501","AUTOMATIC; Caleffi","AIR VENT","3/4 X 3/8 IN","BRASS,INTERNAL: STAINLESS, SEAL :PEAK,NBR FKM","16 BAR","FLOAT TYPE AUTOMATIC","INLET 3/4 NPT FEMALE X EXHAUSE 3/8 NPP FEMALE STRAIGHT","1.5 MM",null,"AIR",null,"120 DEG C",501500,null,"O RING RUBBER"]
["Palmiet Pumped Storage Scheme",727285,"VALVE: TYPE: FREE FLOATING LEVER AIR VENT; VALVE SIZE: 3/4 X 1/2 IN; DESIGN RATING: 21 BAR; TEMPERATURE RATING: 93 DEG C; FACE TO FACE LENGTH: 10.6 MM; CONNECTION: INLET 3/4 OUTLET 1/2 INCH; OPERATED: FLOAT; BODY MATERIAL: CAST IRON; STYLE: BOWL; SOFTGOODS: GRAPHITE GASKET (ITEM 9), 1.4301 WASHER (ITEM 14); MANUF P/N: 1AV ; SEAT, LEVERAGE SYSTEM, FLOAT STAINLESS STEEL, BODY AND CAP ASTM A48 CLASS 30 CAST IRON, GASKET GRAPHITE 60 X 75X 1 MM, BLOTS ASTM A193 GR B7, NUTS ASTM A563 GR A","ARMSTRONG INTERNATIONAL","FREE FLOATING LEVER AIR VENT","3/4 X 1/2 IN","CAST IRON","21 BAR",null,"INLET 3/4 OUTLET 1/2 INCH","10.6 MM",null,"FLOAT",null,"93 DEG C","1AV",null,"GRAPHITE GASKET (ITEM 9), 1.4301 WASHER (ITEM 14); A"]
["Palmiet Pumped Storage Scheme",738906,"KIT, COMPRESSOR REPAIR: TYPE: SERVICE; APPLICATION: SPHERICAL VALVE; SPECIFICATION: ELECTRIC; COMPRISING: PISTON RINGS & GASKETS; MANUF P/N: 32226342; TYPE 30 MODEL 15T2, COMPRESSION STAGES 1, 2 AND 3, INGERSOLL RAND","TYPE 30; Ingersoll Rand","SERVICE",{"$nulls":8},"SPHERICAL VALVE",null,32226342]
["Palmiet Pumped Storage Scheme",751644,"VALVE, BALL: VALVE SIZE: 12 MM; DESIGN RATING: 400 BAR; TEMPERATURE RATING: -10 to +100 DEG C; CONNECTION: 1/2 IN; BODY MATERIAL: CARBON STEEL; FACE TO FACE LENGTH: 100 MM; OPERATED: LEVER; STYLE: SQUARE; TRIM: CARBON STEEL; SOFTGOODS: NONE; SPECIFICATION: 4 WAY BALL; PORT TYPE: STRAIGHT 1/2 INCH FITTING MALE TO FEMALE; APPLICATION: MAINTENANCE SEAL OPERATION","Parker Hannifin ","BALL; STRAIGHT 1/2 INCH FITTING MALE TO FEMALE","12 MM","CARBON STEEL","400 BAR","CARBON STEEL","1/2 IN","100 MM",null,"LEVER","MAINTENANCE SEAL OPERATION","-10 to +100 DEG C",null,null,"NONE"]
["Palmiet Pumped Storage Scheme",751649,"VALVE, BALL: VALVE SIZE: 12 MM; DESIGN RATING: 400 BAR; TEMPERATURE RATING: -10 to +100 DEG C; CONNECTION: 1/2'' STRAIGHT FEMALE FITTING; BODY MATERIAL: CS/CS-CS-POM; FACE TO FACE LENGTH: 100 MM; OPERATED: LEVER; STYLE: 3 WAY; TRIM: CARBON STEEL BALL ELEMENT; SOFTGOODS: NONE; SPECIFICATION: MULTI WAY BALL VALVE; PORT TYPE: 1/2 INCH FULL PORT IN; APPLICATION: OPERATING SEAL OPERATION; TYPE: ARGUS MW8","Argus","BALL; 1/2 INCH FULL PORT IN; ARGUS MW8","12 MM","CS/CS-CS-POM","400 BAR","CARBON STEEL BALL ELEMENT","1/2'' STRAIGHT FEMALE FITTING","100 MM",null,"LEVER","OPERATING SEAL OPERATION","-10 to +100 DEG C",null,null,"NONE"]
["Palmiet Pumped Storage Scheme",783654,"VALVE, GATE: VALVE SIZE: 80 MM; TYPE: GATE; DESIGN PRESSURE: 18 BAR; DESIGN TEMPERATURE: -120 TO 200 DEG C; CONNECTION: FLANGED DRILLED TO BS4504 PN 16; FACE TO FACE LENGTH: 223 MM; BODY MATERIAL: CAST IRON; TRIM: 8; OPERATED: HANDWHEEL; STEM DESIGN: RISING STEM; SPECIAL FEATURES: RESILIENT SEAT VALVE; AINSWORTH ,RAISED FACE,FIRE HYDRANT ,PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY","Ainsworth","GATE","80 MM","CAST IRON","18 BAR","8; RISING STEM","FLANGED DRILLED TO BS4504 PN 16","223 MM",null,"HANDWHEEL",null,"-120 TO 200 DEG C",null,null,"E","PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY; CERTIFICATES TO BE SUPPLIED UPON DELIVERY"]
["Palmiet Pumped Storage Scheme",783433,"VALVE, GATE: VALVE SIZE: 150 MM; TYPE: SOLID WEGDE; DESIGN PRESSURE: 64 BAR; DESIGN TEMPERATURE: -20 to 200 DEG C; CONNECTION: FLANGED; FACE TO FACE LENGTH: 447 MM; BODY MATERIAL: CARBON STEEL; TRIM: 8; OPERATED: MANUAL HANDWHEEL; DIN 3352 T7,SPIRAL CASE DRAINAGE , PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY.","NEWAY","GATE; SOLID WEGDE","150 MM","CARBON STEEL","64 BAR",8,"FLANGED","447 MM",null,"MANUAL HANDWHEEL",null,"-20 to 200 DEG C",{"$nulls":3},"PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY; CERTIFICATES TO BE SUPPLIED UPON DELIVERY"]
["Palmiet Pumped Storage Scheme",783757,"VALVE, DIAPHRAGM: TYPE: A; VALVE SIZE: 15 MM; DESIGN RATING: 16 BAR; TEMPERATURE RATING: -5 TO 100 DEG C; CONNECTION: SCREWED BSP THREADED FEMALE; BODY MATERIAL: CAST IRON; DIAPHRAGM MATERIAL: DIAPHRAGM GRADE Q; FACE TO FACE LENGTH: 64 MM; OPERATED: MANUAL; STYLE: TYPE A; SPECIFICATION: COATED; WATR TREATMENT, SAUNDERS WIER TYPE, SUPPLIER TO PROVIDE WITH THE PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATES.","Saunders","DIAPHRAGM; A","15 MM","CAST IRON; DIAPHRAGM GRADE Q","16 BAR","DIAPHRAGM GRADE Q","SCREWED BSP THREADED FEMALE","64 MM",null,"MANUAL",null,"-5 TO 100 DEG C",{"$nulls":3},"PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATES; CERTIFICATES"]
["Palmiet Pumped Storage Scheme",783432,"VALVE, GATE: VALVE SIZE: 300 MM; TYPE: SOLID WEDGE WITH BYPASS; DESIGN PRESSURE: 63 BAR; DESIGN TEMPERATURE: -20 to 200 DEG C; CONNECTION: FLANGE FLAT FACE WITH O-RING GROOVE; FACE TO FACE LENGTH: 750 MM; BODY MATERIAL: CARBON STEEL; TRIM: 8; OPERATED: HANDWHEEL ACTUATED; STEM DESIGN: RISING STEM; APPLICATION: MANUAL BYPASS ISOLATING VALVE; SPECIAL FEATURES: WITH OPEN / CLOSE LEVEL INDICATOR; MANUF P/N: TYPE B3.35461; PRESSURE TESTING AND MATERIAL CERTIFICATE TO BE SUPPLIED UPON DELIVERY.","B3","GATE; SOLID WEDGE WITH BYPASS","300 MM","CARBON STEEL","63 BAR","8; RISING STEM","FLANGE FLAT FACE WITH O-RING GROOVE","750 MM",null,"HANDWHEEL ACTUATED","MANUAL BYPASS ISOLATING VALVE","-20 to 200 DEG C","TYPE B3.35461",null,null,"PRESSURE TESTING AND MATERIAL CERTIFICATE TO BE SUPPLIED UPON DELIVERY; CERTIFICATE TO BE SUPPLIED UPON DELIVERY"]
["Palmiet Pumped Storage Scheme",783755,"VALVE, BALL: VALVE SIZE: 12 MM; DESIGN RATING: 500 BAR; TEMPERATURE RATING: -45 TO 121 DEG C; CONNECTION: SCREWED TO BDP THREADED FEMALE; BODY MATERIAL: CARBON STEEL; FACE TO FACE LENGTH: 80 MM; OPERATED: MANUAL; TYPE: 2- WAY BALL VALVE; GOVE RECEIVER, PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATES.","Parker Hannifin ","BALL; 2- WAY BALL VALVE","12 MM","CARBON STEEL","500 BAR",null,"SCREWED TO BDP THREADED FEMALE","80 MM",null,"MANUAL",null,"-45 TO 121 DEG C",{"$nulls":3},"PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATES; CERTIFICATES"]
["Palmiet Pumped Storage Scheme",783664,"VALVE: TYPE: 2-WAY; VALVE SIZE: 20 MM; DESIGN RATING: 420 BAR; TEMPERATURE RATING: -10 TO 80 DEG C; FACE TO FACE LENGTH: 95 MM; CONNECTION: SCREWED TO BSP THREADED FEMALE; OPERATED: MANUAL; BODY MATERIAL: CARBON STEEL; STYLE: BLOCK TYPE; GOV REC, THREADED FEMALE, SUPPLIER TO SUPPLY WITH THE PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATES.","Parker Hannifin/ HYDAC","2-WAY","20 MM","CARBON STEEL","420 BAR",null,"SCREWED TO BSP THREADED FEMALE","95 MM",null,"MANUAL",null,"-10 TO 80 DEG C",{"$nulls":3},"PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATES; CERTIFICATES"]
["Palmiet Pumped Storage Scheme",783762,"VALVE, DIAPHRAGM: TYPE: A; VALVE SIZE: 25 MM; DESIGN RATING: 16 BAR; TEMPERATURE RATING: -5 TO 100 DEG C; CONNECTION: SCREWED TO BSP THREADED FEMALE; BODY MATERIAL: CAST IRON; DIAPHRAGM MATERIAL: GRADE 1; FACE TO FACE LENGTH: 108 MM; OPERATED: MANUAL; STYLE: TYPE A; SPECIFICATION: COATED; WATER TREATMENT, SAUNDERS WEIR TYPE, Q DIAPHRAGM, SUPPLIER TO SUPPLY WITH THE PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATES.","Saunders","DIAPHRAGM; A","25 MM","CAST IRON; GRADE 1","16 BAR","GRADE 1","SCREWED TO BSP THREADED FEMALE","108 MM",null,"MANUAL",null,"-5 TO 100 DEG C",{"$nulls":3},"PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATES; CERTIFICATES"]
["Palmiet Pumped Storage Scheme",750298,"VALVE, RELIEF: VALVE SIZE: G3/4; SET PRESSURE: 48.5 BAR; TEMPERATURE RATING: -15 TO 200 DEG C; CONNECTION: G3/4 IN; BODY MATERIAL: BRASS; TRIM: BRASS; OPERATED: PRESSURE SPRING LOADED; MANUF P/N: PSB013-075; SAFETY VALVE TO BE SET AT 11 BAR (COLD SET PRESSURE). SAFETY VALVE TO BE TAGGED AND LED SEALED. INFORMATION ON TAG SHOULD CONTAIN:VALVE SERIAL NUMBER, SET PRESSURE, TEST DATE AND DUE DATE. DUE DATE SHOULD BE 3 YEARS FROM TEST DATE. VALVE. TEST REPORT TO BE SUPPLIED ALONG WITH VALVE.TEST REPORT TO DETAIL TO CORRESPOND WITH VALVE INFO","LESER","RELIEF","G3/4","BRASS","48.5 BAR","BRASS","G3/4 IN",null,null,"PRESSURE SPRING LOADED",null,"-15 TO 200 DEG C","PSB013-075",null,null,"TEST REPORT TO BE SUPPLIED ALONG WITH VALVE; TEST REPORT TO DETAIL TO CORRESPOND WITH VALVE INFO"]
["Palmiet Pumped Storage Scheme",783431,"VALVE: TYPE: PLUG; VALVE SIZE: 300 MM; DESIGN RATING: 50 BAR; TEMPERATURE RATING: -20 to 200 DEG C; CONNECTION: FLANGED FLAT FACE WITH O-RING GROOVE; OPERATED: HYDRAULIC; BODY MATERIAL: CARBON STEEL; TRIM: 8; MANUF P/N: 2.53-18555; SPHERICAL VALVE BYPASS VALVE.PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY","NEWAY","PLUG","300 MM","CARBON STEEL","50 BAR",8,"FLANGED FLAT FACE WITH O-RING GROOVE",null,null,"HYDRAULIC",null,"-20 to 200 DEG C","2.53-18555",null,null,"PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY; CERTIFICATES TO BE SUPPLIED UPON DELIVERY"]
["Palmiet Pumped Storage Scheme",783759,"VALVE, DIAPHRAGM: TYPE: A; VALVE SIZE: 50 MM; DESIGN RATING: 16 BAR; TEMPERATURE RATING: -5 TO 100 DEG C; CONNECTION: SCREWED T BSP THREADED FEMALE; BODY MATERIAL: CAST IRON; DIAPHRAGM MATERIAL: DIAPHRAGM GRADE Q; FACE TO FACE LENGTH: 165 MM; OPERATED: MANUAL; STYLE: TYPE A; SPECIFICATION: COATED; WATER TREATMENT, SAUNDERS WEIR TYPE, Q DIAPHRAGM, SUPPLIER TO SUPPLY WITH THE PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATES","Saunders","DIAPHRAGM; A","50 MM","CAST IRON; DIAPHRAGM GRADE Q","16 BAR","DIAPHRAGM GRADE Q","SCREWED T BSP THREADED FEMALE","165 MM",null,"MANUAL",null,"-5 TO 100 DEG C",{"$nulls":3},"PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATES; CERTIFICATES"]
["Palmiet Pumped Storage Scheme",765642,"VALVE, GATE: VALVE SIZE: 100 MM; TYPE: SOLID WEDGE; DESIGN PRESSURE: 64 BAR; DESIGN TEMPERATURE: -20 to +400 DEG C; CONNECTION: FLANGED DIN 2513 FEMALE JOINT FLANGE ENDS; FACE TO FACE LENGTH: 350 MM; BODY MATERIAL: STAINLESS STEEL 304; TRIM: BODY SS304 ; BONNET SS304 ; WEDGE : SS304 ; SEAT : SS304 ; STEM : SS304; OPERATED: HANDWHEEL RISING SPINDLE; APPLICATION: PALMIET LABYRINTH SUPPLY ISOLATION; SPECIFICATION: DESIGN AS PER DIN3352 / EN1171; SPECIAL FEATURES: TO BE SUPPLIED WITH PRESSURE TEST AND MATERIAL CERTIFICATES; GRADE: STAINLESS STEEL 304","DATA NOT AVAILABLE","GATE; SOLID WEDGE","100 MM","STAINLESS STEEL 304","64 BAR","BODY SS304","FLANGED DIN 2513 FEMALE JOINT FLANGE ENDS","350 MM",null,"HANDWHEEL RISING SPINDLE","PALMIET LABYRINTH SUPPLY ISOLATION","-20 to +400 DEG C",null,null,"SS304","PRESSURE TEST AND MATERIAL CERTIFICATES; CERTIFICATES"]
["Palmiet Pumped Storage Scheme",780490,"MANIFOLD: TYPE: 2 WAY VALVE MANIFOLD; MATERIAL: STAINLESS STEEL; MANUF P/N: P2/W4GW4GTV2AH-R; 2 VALVE BLOCK AND VENT GAUGE VALVE, PROCESS CONNECTION FEMALE 1/2” BSPG, INSTRUMENT CONNECTION FEMALE 1/2” BSPG, PTFE PACKING,1/4” NPT VENT PORT, ALL TAPS ANTI-TAMPER, 6000 PSI, 316 SS, M6 X 16MM PCD MOUNTING HOLES; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","No further information available","PROCESS CONNECTION FEMALE 1/2” BSPG, INSTRUMENT CONNECTION FEMALE 1/2” BSPG, PTFE PACKING,1/4” NPT VENT PORT, ALL TAPS ANTI-TAMPER, 6000 PSI, 316 SS, M6 X 16MM PCD MOUNTING HOLES; 2 WAY VALVE MANIFOLD",null,"STAINLESS STEEL",{"$nulls":4},"MOUNTING HOLES",{"$nulls":3},"P2/W4GW4GTV2AH-R"]
["Palmiet Pumped Storage Scheme",783419,"VALVE, GATE: VALVE SIZE: 50 MM; TYPE: GATE VALVE; DESIGN PRESSURE: 10 BAR; DESIGN TEMPERATURE: -29 TO 400 DEG C; CONNECTION: FLANGE DRILLED TO JIS 10K50; FACE TO FACE LENGTH: 140 MM; BODY MATERIAL: FCMB-535; TRIM: TRIM 8; OPERATED: MANUAL; HP INLET, GATE VALVE, SUPPLIER TO PROVE PRESSURE TEST CERTIFICATE AND THE MATERIAL PROPERTIES ON DELIVERY.","MALL","GATE; SUPPLIER TO PROVE PRESSURE TEST CERTIFICATE AND THE MATERIAL PROPERTIES ON DELIVERY; GATE VALVE","50 MM","FCMB-535","10 BAR","TRIM 8","FLANGE DRILLED TO JIS 10K50","140 MM",null,"MANUAL",null,"-29 TO 400 DEG C",{"$nulls":3},"PRESSURE TEST CERTIFICATE AND THE MATERIAL PROPERTIES ON DELIVERY; CERTIFICATE AND THE MATERIAL PROPERTIES ON DELIVERY"]
["Palmiet Pumped Storage Scheme",783758,"VALVE, DIAPHRAGM: TYPE: A; VALVE SIZE: 40 MM; DESIGN RATING: 16 BAR; TEMPERATURE RATING: -5 TO 100 DEG C; CONNECTION: FLANGE DRILLED TO BS4504 T16; BODY MATERIAL: CAST IRON; DIAPHRAGM MATERIAL: DIAPHRAGM GRADE Q; FACE TO FACE LENGTH: 165 MM; OPERATED: MANUAL; STYLE: TYPE A; SPECIFICATION: COATED; WATER TREATMENT, SAUNDERS WEIR TYPE, Q DIAPHRAGM, SUPPLIER TO SUPPLY WITH THE PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATES","Saunders","DIAPHRAGM; A","40 MM","CAST IRON; DIAPHRAGM GRADE Q","16 BAR","DIAPHRAGM GRADE Q","FLANGE DRILLED TO BS4504 T16","165 MM",null,"MANUAL",null,"-5 TO 100 DEG C",{"$nulls":3},"PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATES; CERTIFICATES"]
["Palmiet Pumped Storage Scheme",780491,"MANIFOLD: TYPE: 3 VALVE DIRECT MOUNT MANIFOLD; MATERIAL: STAINLESS STEEL; MANUF P/N: S3/FTHAX-ZH; 3 WAY DIRECT MOUNT MANIFOLD, PTFE PACKING AND GASKET, 6000 PSI, 316 SS, ALL TAPS ANTI-TAMPER, O-RING TX HOOK-UP, 316 SS ASSEMBLY BOLT KIT INCLUDED; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","No further information available","3 VALVE DIRECT MOUNT MANIFOLD",null,"STAINLESS STEEL",{"$nulls":8},"S3/FTHAX-ZH"]
["Palmiet Pumped Storage Scheme",783503,"VALVE, GLOBE: VALVE SIZE: 80 MM; DESIGN PRESSURE: 2 - 21 BAR; DESIGN TEMPERATURE: 82 DEG C; FACE TO FACE LENGTH: 336 MM; OPERATED: SELF OPERATED; CONNECTION: FLANGE DRILLED TO BS4504 T16; BODY MATERIAL: STAINLESS STEEL; TRIM: STAINLESS STEEL; TYPE: PRESURE REDUCING GLOBE VALVE; MANUF P/N: 20868931A; OIL PURIFY BYPASS, PRESSURE REDUCING VALVE, FLANGE THICKNESS: 30MM, 8 BOLTS, CLA-VAL.CO, THIS VALVE INCLUDE 1 PRESSURE GAUGE, SST CRD PILOT AND TRIM & POSITION INDICATOR, SUPPLIER TO PROVIDE THE FOLLOWING ON DELIVERY: PRESURE TEST CERTIFICATE & MATERIAL PROPERTIES CERTIFICATE.","CLA-VAL.CO","GLOBE; FLANGE THICKNESS; PRESURE REDUCING GLOBE VALVE","80 MM","STAINLESS STEEL","2 - 21 BAR","STAINLESS STEEL","FLANGE DRILLED TO BS4504 T16","336 MM",null,"SELF OPERATED",null,"82 DEG C","20868931A",null,null,"CERTIFICATE & MATERIAL PROPERTIES CERTIFICATE"]
["Palmiet Pumped Storage Scheme",683354,"FLANGE: TYPE: DIESEL ENGINE AIR STARTING VALVE; DIMENSIONS: OD 152.4 MM; MATERIAL: CARBON STEEL; STYLE: RAISED FACE; GRADE: 304; SPECIFICATION: SABS 1123 1600/3; RAISED FACE = 3MM, OD = 152.4MM, ID = TO SUIT 50NB PIPE, PCD = 120.6MM, FLANGE THICKNESS = 25MM, NUMBER OF HOLES = 4, DIAMETER OF BOLT HOLES = 18MM","No further information available","DIESEL ENGINE AIR STARTING VALVE",null,"CARBON STEEL"]
["Palmiet Pumped Storage Scheme",783425,"VALVE, CHECK: TYPE: CHECK VALVE; VALVE SIZE: 100 MM; DESIGN RATING: 40 BAR; TEMPERATURE RATING: -20 TO 120 DEG C; CONNECTION: FLANGE DRILLED TO BS4504 TABLE 40; BODY MATERIAL: WCB; FACE TO FACE LENGTH: 344 MM; OPERATED: SELF (SWING CHECK); BLOWDOWN AIR NON-RETURN VALVE, PERSTA, MODEL 240MT11.1, PRESSURE TESTING AND MATERIAL PROPERTIES TO SUPPLIED ON DELIVERY BY THE SUPPLIER.","PERSTA","CHECK; PERSTA, MODEL 240MT11.1, PRESSURE TESTING AND MATERIAL PROPERTIES TO SUPPLIED ON DELIVERY BY THE SUPPLIER; CHECK VALVE","100 MM","WCB","40 BAR",null,"FLANGE DRILLED TO BS4504 TABLE 40","344 MM",null,"SELF (SWING CHECK)",null,"-20 TO 120 DEG C",{"$nulls":3},"PRESSURE TESTING AND MATERIAL PROPERTIES TO SUPPLIED ON DELIVERY BY THE SUPPLIER"]
["Palmiet Pumped Storage Scheme",783437,"VALVE: TYPE: GLOBE; VALVE SIZE: 100 MM; DESIGN RATING: 64 BAR; TEMPERATURE RATING: -20 TO 200 DEG C; FACE TO FACE LENGTH: 430 MM; CONNECTION: FLANGED & DRILLED TO EN1092-1; OPERATED: HYDRAULIC ACTUATOR WITH OPEN AND CLOSED POSITION SWITCH; BODY MATERIAL: CARBON STEEL; TRIM: 8; MANUF P/N: 2.41-48223; LABYRINTH COOLING WATER HYDRAULIC VALVE , PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY.","DATA NOT AVAILABLE","GLOBE","100 MM","CARBON STEEL","64 BAR",8,"FLANGED & DRILLED TO EN1092-1","430 MM",null,"HYDRAULIC ACTUATOR WITH OPEN AND CLOSED POSITION SWITCH",null,"-20 TO 200 DEG C","2.41-48223",null,null,"PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY; CERTIFICATES TO BE SUPPLIED UPON DELIVERY"]
["Palmiet Pumped Storage Scheme",783422,"VALVE, GLOBE: VALVE SIZE: 50 MM; DESIGN PRESSURE: 40 BAR; DESIGN TEMPERATURE: -196 to 573 DEG C; FACE TO FACE LENGTH: 224 MM; OPERATED: MANUAL; CONNECTION: FLANGE DRILLED TO EN1092-1 TABLE 40; BODY MATERIAL: STAINLESS STEEL; TRIM: STAINLESS STEEL; INNER AND OUTER LAYBYRINTH, RAISED FACE WITH O-RING GROOVE, NON-RISING STEM, 200AF211, 1.0460, PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATE ON DELIVERY.","DATA NOT AVAILABLE","GLOBE","50 MM","STAINLESS STEEL","40 BAR","STAINLESS STEEL","FLANGE DRILLED TO EN1092-1 TABLE 40","224 MM",null,"MANUAL",null,"-196 to 573 DEG C",{"$nulls":3},"PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATE ON DELIVERY; CERTIFICATE ON DELIVERY"]
["Palmiet Pumped Storage Scheme",783760,"VALVE, DIAPHRAGM: TYPE: A; VALVE SIZE: 80 MM; DESIGN RATING: 16 BAR; TEMPERATURE RATING: -5 to 100 DEG; CONNECTION: FLANGE DRILLED TO BS4504 T16; BODY MATERIAL: CAST IRON; DIAPHRAGM MATERIAL: DIAPHRAGM GRADE Q; FACE TO FACE LENGTH: 260 MM; OPERATED: MANUAL; STYLE: TYPE A; SPECIFICATION: COATED; WATER TREATMENT, SAUNDERS WEIR TYPE, Q DIAPHRAGM, SUPPLIER TO SUPPLY WITH THE PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATES","Saunders","DIAPHRAGM; A","80 MM","CAST IRON; DIAPHRAGM GRADE Q","16 BAR","DIAPHRAGM GRADE Q","FLANGE DRILLED TO BS4504 T16","260 MM",null,"MANUAL",null,"-5 to 100 DEG",{"$nulls":3},"PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATES; CERTIFICATES"]
["Palmiet Pumped Storage Scheme",783426,"VALVE, BALL: VALVE SIZE: 80 MM; DESIGN RATING: 40 BAR; TEMPERATURE RATING: -40 TO 200 DEG C; CONNECTION: FLANGE DRILLED TO EN1092-1; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 180 MM; OPERATED: MANUAL; LEVEL INDICATOR L5 DRAFT TUBE, MODENTIC MD-27, DIN2635, RAISED FACE, PRESSURE TEST CERTIFICATE AND MATERIAL PROPERTIES CERTIFICATE TO BE SUPPLIED ON DELIVERY.","stewartsandlloydsvalves","BALL","80 MM","STAINLESS STEEL","40 BAR",null,"FLANGE DRILLED TO EN1092-1","180 MM",null,"MANUAL",null,"-40 TO 200 DEG C",{"$nulls":3},"PRESSURE TEST CERTIFICATE AND MATERIAL PROPERTIES CERTIFICATE TO BE SUPPLIED ON DELIVERY; CERTIFICATE AND MATERIAL PROPERTIES CERTIFICATE TO BE SUPPLIED ON DELIVERY"]
["Palmiet Pumped Storage Scheme",783761,"VALVE, DIAPHRAGM: TYPE: A; VALVE SIZE: 20 MM; DESIGN RATING: 16 BAR; TEMPERATURE RATING: -5 TO 100 DEG C; CONNECTION: SCREWED TO BSP THREADED FEMALE; BODY MATERIAL: CAST IRON; DIAPHRAGM MATERIAL: GRADE Q; FACE TO FACE LENGTH: 83 MM; OPERATED: MANUAL; STYLE: TYPE A; SPECIFICATION: COATED; WATER TREATMENT, SAUNDERS WEIR TYPE, Q DIAPHRAGM, SUPPLIER TO SUPPLY WITH THE PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATES","Saunders","DIAPHRAGM; A","20 MM","CAST IRON; GRADE Q","16 BAR","GRADE Q","SCREWED TO BSP THREADED FEMALE","83 MM",null,"MANUAL",null,"-5 TO 100 DEG C",{"$nulls":3},"PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATES; CERTIFICATES"]
["Palmiet Pumped Storage Scheme",783505,"VALVE, BALL: VALVE SIZE: 50 MM; DESIGN RATING: 19 BAR; TEMPERATURE RATING: 5 - 75 DEG C; CONNECTION: FLANGED DRILLED TO BS4504 T16; BODY MATERIAL: WCB; FACE TO FACE LENGTH: 178 MM; OPERATED: MANUAL; TRIM: STAINLESS STEEL; TYPE: REDUCED BORE; OIL PURIFY, REDUCED BORE VALL VALE, CLASS 150, SERIES 500 BALL VALVE, IPVI, SUPPLIER TO PROVIDE WITH THE PRESSURE TEST CERTIFICATE AND A MATERIAL PROPERTIES CERTIFICATE.","IPV","BALL; IPVI, SUPPLIER TO PROVIDE WITH THE PRESSURE TEST CERTIFICATE AND A MATERIAL PROPERTIES CERTIFICATE; REDUCED BORE","50 MM","WCB","19 BAR","STAINLESS STEEL","FLANGED DRILLED TO BS4504 T16","178 MM",null,"MANUAL",null,"5 - 75 DEG C",{"$nulls":3},"PRESSURE TEST CERTIFICATE AND A MATERIAL PROPERTIES CERTIFICATE; CERTIFICATE AND A MATERIAL PROPERTIES CERTIFICATE"]
["Palmiet Pumped Storage Scheme",783430,"VALVE: TYPE: GLOBE; VALVE SIZE: 100 MM; DESIGN RATING: 40 BAR; TEMPERATURE RATING: -20 to 200 DEG C; FACE TO FACE LENGTH: 340 MM; CONNECTION: FLANGED DRILLED TO BS4504 TABLE 40; OPERATED: MANUAL HANDWHEEL; BODY MATERIAL: CARBON STEEL; TRIM: 8; BLOWDOWN AIR RECEIVER ISOLATION VALVE , PRESSURE TESTING AND MATERIAL CERTIDFICATES TO BE SUPPLIED UPON DELIVERY.","DATA NOT AVAILABLE","GLOBE","100 MM","CARBON STEEL","40 BAR",8,"FLANGED DRILLED TO BS4504 TABLE 40","340 MM",null,"MANUAL HANDWHEEL",null,"-20 to 200 DEG C",{"$nulls":3},"PRESSURE TESTING AND MATERIAL CERTIDFICATES TO BE SUPPLIED UPON DELIVERY"]
["Palmiet Pumped Storage Scheme",783427,"VALVE: TYPE: PLUG; VALVE SIZE: 40 MM; DESIGN RATING: 100 BAR; TEMPERATURE RATING: -20 to 200 DEG C; CONNECTION: FLANGED DRILLED TO EN1092-1; OPERATED: HYDRAULIC ACTUATOR WITH OPEN AND CLOSED POSITION SWITCH; BODY MATERIAL: CARBON STEEL; TRIM: 8; MANUF P/N: 2.41-48231; PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY.SHAFT SEAL HYDRAULIC VALVE","DATA NOT AVAILABLE","PLUG","40 MM","CARBON STEEL","100 BAR",8,"FLANGED DRILLED TO EN1092-1",null,null,"HYDRAULIC ACTUATOR WITH OPEN AND CLOSED POSITION SWITCH",null,"-20 to 200 DEG C","2.41-48231",null,null,"PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY; CERTIFICATES TO BE SUPPLIED UPON DELIVERY"]
["Palmiet Pumped Storage Scheme",768522,"VALVE, GLOBE: VALVE SIZE: 15 MM; DESIGN PRESSURE: 10 KG/CM2; DESIGN TEMPERATURE: 180 DEG C; FACE TO FACE LENGTH: 85 MM; OPERATED: HANDWHEEL; CONNECTION: FLANGE; BODY MATERIAL: SCS13; TRIM: 18CR-8NI; SPECIFICATION: 10K-15 , KITZ , GLOBE VALVE","KITS","GLOBE","15 MM","SCS13","10 KG/CM2","18CR-8NI","FLANGE","85 MM",null,"HANDWHEEL",null,"180 DEG C"]
["Palmiet Pumped Storage Scheme",783792,"VALVE, GATE: VALVE SIZE: 250 MM; TYPE: SOLID WEDGE; DESIGN PRESSURE: 16 BAR; DESIGN TEMPERATURE: 5 TO 40 DEG C; CONNECTION: FLANGED DRILLED TO BS4504 T16; FACE TO FACE LENGTH: 356 MM; BODY MATERIAL: CAST STEEL; TRIM: GUNMETAL; OPERATED: MANUAL HANDWHEEL; SPECIAL FEATURES: COPON LINED; DEWATERING, AINSWORTH RESILIENT SEAL GATE VALVE, NON-RISING SPINDLE WITH POSITION INDICATOR, PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATE TO BE SUPPLIED BY THE SUPPLIER ON DELIVERY.","Ainsworth","GATE; NON-RISING SPINDLE WITH POSITION INDICATOR, PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATE TO BE SUPPLIED BY THE SUPPLIER ON DELIVERY; SOLID WEDGE","250 MM","CAST STEEL","16 BAR","GUNMETAL","FLANGED DRILLED TO BS4504 T16","356 MM",null,"MANUAL HANDWHEEL",null,"5 TO 40 DEG C",{"$nulls":3},"PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATE TO BE SUPPLIED BY THE SUPPLIER ON DELIVERY; CERTIFICATE TO BE SUPPLIED BY THE SUPPLIER ON DELIVERY"]
["Palmiet Pumped Storage Scheme",783434,"VALVE, GATE: VALVE SIZE: 300 MM; TYPE: SOLID WEDGE; DESIGN PRESSURE: 25 BAR; DESIGN TEMPERATURE: -20 to 200 DEG C; CONNECTION: FLANGED , DRILLED TO BS4504 PN25; FACE TO FACE LENGTH: 345 MM; BODY MATERIAL: CARBON STEEL; TRIM: 8; OPERATED: MANUAL HANDWHEEL; SPECIAL FEATURES: INTERNAL EPOXY COATED TO 400 UM; MANUF P/N: D300TS564CSEPO; UNIT CW , PRESSURE TESTING AND MATERIAL CERTIIFICATES TO BE SUPPLIED UPON DELIVERY.","DATA NOT AVAILABLE","GATE; SOLID WEDGE","300 MM","CARBON STEEL","25 BAR",8,"FLANGED , DRILLED TO BS4504 PN25","345 MM",null,"MANUAL HANDWHEEL",null,"-20 to 200 DEG C","D300TS564CSEPO",null,null,"PRESSURE TESTING AND MATERIAL CERTIIFICATES TO BE SUPPLIED UPON DELIVERY"]
["Palmiet Pumped Storage Scheme",750300,"VALVE, RELIEF: VALVE SIZE: DN 25; SET PRESSURE: 16.9 BAR; TEMPERATURE RATING: -15/200 DEG C; CONNECTION: 1\" BSP; BODY MATERIAL: BRASS; TRIM: BRASS; OPERATED: AUTOMATIC RELIEF AT SET PRESSURE; MANUF P/N: PSB013-074; SAFETY VALVE TO BE SET AT 16.94 BAR (COLD SET PRESSURE). SAFETY VALVE TO BE TAGGED AND LED SEALED. INFORMATION ON TAG SHOULD CONTAIN: VALVE SERIAL NUMBER, SET PRESSURE, TEST DATE AND DUE DATE. DUE DATE SHOULD BE 3 YEARS FROM TEST DATE. VALVE. TEST REPORT TO BE SUPPLIED ALONG WITH VALVE.TEST REPORT TO DETAIL TO CORRESPOND WITH VALVE INFO. TO SUIT 2ND STAGE ON COMPRESSOR MODEL V250-12-3N","TO SUIT 2ND STAGE ON COMPRESSOR","RELIEF","DN 25","BRASS","16.9 BAR","BRASS","1\" BSP",null,null,"AUTOMATIC RELIEF AT SET PRESSURE",null,"-15/200 DEG C","PSB013-074",null,null,"TEST REPORT TO BE SUPPLIED ALONG WITH VALVE; TEST REPORT TO DETAIL TO CORRESPOND WITH VALVE INFO"]
["Palmiet Pumped Storage Scheme",783756,"VALVE, BALL: VALVE SIZE: 25 MM; DESIGN RATING: 420 BAR; TEMPERATURE RATING: -4 TO 121 DEG; CONNECTION: SCREWED TO BSP THREADED FEMALE; BODY MATERIAL: CARBON STEEL; FACE TO FACE LENGTH: 110 MM; OPERATED: MANUAL; GOV REC, THREADED FEMALE, PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATES TO BE SUPPLIED.","ARGUS","BALL","25 MM","CARBON STEEL","420 BAR",null,"SCREWED TO BSP THREADED FEMALE","110 MM",null,"MANUAL",null,"-4 TO 121 DEG",{"$nulls":3},"PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATES TO BE SUPPLIED; CERTIFICATES TO BE SUPPLIED"]
["Palmiet Pumped Storage Scheme",783435,"VALVE: TYPE: PLUG; VALVE SIZE: 150 MM; DESIGN RATING: 64 BAR; TEMPERATURE RATING: -20 to 200 DEG C; CONNECTION: FLANGED & DRILLED TO EN1092-1; OPERATED: HYDRAULIC ACTUATOR WITH OPEN AND CLOSED POSITION SWITCH; BODY MATERIAL: CARBON STEEL; MANUF P/N: 2.41-48660; RUNNER BAND DRAIN HYDRAULIC VALVES , PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY","VOITH","PLUG","150 MM","CARBON STEEL","64 BAR",null,"FLANGED & DRILLED TO EN1092-1",null,null,"HYDRAULIC ACTUATOR WITH OPEN AND CLOSED POSITION SWITCH",null,"-20 to 200 DEG C","2.41-48660",null,null,"PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY; CERTIFICATES TO BE SUPPLIED UPON DELIVERY"]
["Palmiet Pumped Storage Scheme",783423,"VALVE, GATE: VALVE SIZE: 200 MM; TYPE: GATE VALVE; DESIGN PRESSURE: 10 BAR; DESIGN TEMPERATURE: -40 to 120 DEG C; CONNECTION: FLANGED; FACE TO FACE LENGTH: 290 MM; BODY MATERIAL: DUCTILE IRON; TRIM: STAINLESS STEEL; OPERATED: MANUAL; TGB ISOLATOR OIL, WORM & WHEEL GEAR STEM HANDLE WITH POSITION INDICATOR, RAISED FACE, BA-04P-P/N, SUMPLIER TO PROVIDE WITH THE PRESSURE TESTING & MATERIAL PROPERTIES CERTIFICATES.","DATA NOT AVAILABLE","GATE; GATE VALVE","200 MM","DUCTILE IRON","10 BAR","STAINLESS STEEL","FLANGED","290 MM",null,"MANUAL",null,"-40 to 120 DEG C",{"$nulls":3},"PRESSURE TESTING & MATERIAL PROPERTIES CERTIFICATES; CERTIFICATES"]
["Palmiet Pumped Storage Scheme",783754,"VALVE, BALL: VALVE SIZE: 06 MM; DESIGN RATING: 500 BAR; TEMPERATURE RATING: -20 TO 60 DEG C; CONNECTION: THREADED FEMALE; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 70 MM; OPERATED: MANUAL; GOV COMPRESSOR BALL VALVE, PRESSURE TEST AND MATERIAL PROPERTIES","PERSTA","BALL; PRESSURE TEST AND MATERIAL PROPERTIES","06 MM","STAINLESS STEEL","500 BAR",null,"THREADED FEMALE","70 MM",null,"MANUAL",null,"-20 TO 60 DEG C",{"$nulls":3},"PRESSURE TEST AND MATERIAL PROPERTIES"]
["Palmiet Pumped Storage Scheme",783421,"VALVE, GATE: VALVE SIZE: 32 MM; TYPE: GATE VALVE; DESIGN PRESSURE: 10 BAR; DESIGN TEMPERATURE: -29 to 425 DEG C; CONNECTION: FLANGE DRILLED TO JIS 10K50; FACE TO FACE LENGTH: 120 MM; BODY MATERIAL: FCMB-535; TRIM: TRIM 8; OPERATED: MANUAL; HP OUTLET VALVE, PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATE ON DELIVERY.","MALL","GATE; PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATE ON DELIVERY; GATE VALVE","32 MM","FCMB-535","10 BAR","TRIM 8","FLANGE DRILLED TO JIS 10K50","120 MM",null,"MANUAL",null,"-29 to 425 DEG C",{"$nulls":3},"PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATE ON DELIVERY; CERTIFICATE ON DELIVERY"]
["Palmiet Pumped Storage Scheme",684520,"VALVE: TYPE: SCREW DOWN NON-RETURN; VALVE SIZE: 1 IN; DESIGN RATING: 38 BAR; TEMPERATURE RATING: 100 DEG C; FACE TO FACE LENGTH: 241 MM; CONNECTION: FLANGED ENDS TO ANSI-300 LB; OPERATED: SWING, DISK; BODY MATERIAL: FORGED STEEL; STYLE: FLANGE BOLTED; TRIM: PLATNAM; SPECIFICATION: ANSI-300 LB (ASA); SOFTGOODS: GRAPHITE; SWING DISK","DATA NOT AVAILABLE","SCREW DOWN NON-RETURN","1 IN","FORGED STEEL","38 BAR","PLATNAM","FLANGED ENDS TO ANSI-300 LB","241 MM",null,"SWING, DISK",null,"100 DEG C",null,null,"GRAPHITE"]
["Palmiet Pumped Storage Scheme",783436,"VALVE: TYPE: GLOBE; VALVE SIZE: 65 MM; DESIGN RATING: 16 BAR; TEMPERATURE RATING: -20 to 200 DEG C; FACE TO FACE LENGTH: 288 MM; CONNECTION: FLANGED , DRILLED TO BS4504 TABLE 16; OPERATED: MANUAL HANDWHEEL; BODY MATERIAL: CARBON STEEL; TRIM: 8; PT GUIDE BEARING OIL ISOLATING VALVES , PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY.","DATA NOT AVAILABLE","GLOBE","65 MM","CARBON STEEL","16 BAR",8,"FLANGED , DRILLED TO BS4504 TABLE 16","288 MM",null,"MANUAL HANDWHEEL",null,"-20 to 200 DEG C",{"$nulls":3},"PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY; CERTIFICATES TO BE SUPPLIED UPON DELIVERY"]
["Palmiet Pumped Storage Scheme",783424,"VALVE, GLOBE: VALVE SIZE: 25 MM; DESIGN PRESSURE: 40 BAR; DESIGN TEMPERATURE: -20 TO 120 DEG C; FACE TO FACE LENGTH: 155 MM; OPERATED: MANUAL; CONNECTION: FLANGE DRILLED TO BS4504 TYPE 40/2; BODY MATERIAL: STAINLESS STEEL; TRIM: STAINLESS STEEL; SHAFT SEAL VALVE, GLOBE VALVE, NON-RISING STEM, RAISED FACE, MODEL:200AE85.1, PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATE ON DELIVERY.","DATA NOT AVAILABLE","GLOBE; GLOBE VALVE, NON-RISING STEM, RAISED FACE, MODEL","25 MM","STAINLESS STEEL","40 BAR","STAINLESS STEEL","FLANGE DRILLED TO BS4504 TYPE 40/2","155 MM",null,"MANUAL",null,"-20 TO 120 DEG C",{"$nulls":3},"PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATE ON DELIVERY; CERTIFICATE ON DELIVERY"]
["Palmiet Pumped Storage Scheme",783504,"VALVE, GLOBE: VALVE SIZE: 100 MM; DESIGN PRESSURE: 16 BAR; DESIGN TEMPERATURE: 400 DEG; FACE TO FACE LENGTH: 230 MM; OPERATED: MANUAL; CONNECTION: FLANGED DRILLED TO BS4504 T16; BODY MATERIAL: STAINLESS STEEL; TRIM: STAINLESS STEEL; MANUF P/N: GMK-GV-DN100-PN16-F2-WCB; TGB COOLER CW INLET & OUTLET VALVE, METAL VALVES(GMK), DIN3356, PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATES TO BE SUPPLIED ON DELIVERY.","GMK","GLOBE; METAL VALVES(GMK), DIN3356, PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATES TO BE SUPPLIED ON DELIVERY","100 MM","STAINLESS STEEL","16 BAR","STAINLESS STEEL","FLANGED DRILLED TO BS4504 T16","230 MM",null,"MANUAL",null,"400 DEG","GMK-GV-DN100-PN16-F2-WCB",null,null,"PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATES TO BE SUPPLIED ON DELIVERY; CERTIFICATES TO BE SUPPLIED ON DELIVERY"]
["Palmiet Pumped Storage Scheme",783650,"VALVE: TYPE: BELLOWS SEAL GLOBE; VALVE SIZE: 1/2 IN; DESIGN RATING: 30 KGF/CM2; TEMPERATURE RATING: -30 to 120 DEG C; FACE TO FACE LENGTH: 58 MM; CONNECTION: THREADED FEMALE ENDS; OPERATED: HANDWHEEL; BODY MATERIAL: BRASS; MANUF P/N: NBV1003; BRAKE AIR COMPRESSOR ,PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY","DATA NOT AVAILABLE","BELLOWS SEAL GLOBE","1/2 IN","BRASS","30 KGF/CM2",null,"THREADED FEMALE ENDS","58 MM",null,"HANDWHEEL",null,"-30 to 120 DEG C","NBV1003",null,null,"PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY; CERTIFICATES TO BE SUPPLIED UPON DELIVERY"]
["Palmiet Pumped Storage Scheme",774960,"KIT: TYPE: PRESSURE RELIEF VALVES; APPLICATION: STANDBY DIESEL GENERAOTR; COMPRISING: PRESSURE RELIEF VALVE (15 BAR, 6-OFF);GROUP 015 TABLE 2/277-1;PART NUMBER:550 180 10 15,PRESSURE RELIEF VALVE (3-OFF);GROUP 016 TABLE 1/589-1;PART NUMBER:550 180 12 15.","DATA NOT AVAILABLE","PRESSURE RELIEF VALVES",{"$nulls":8},"STANDBY DIESEL GENERAOTR"]
["Palmiet Pumped Storage Scheme",783663,"VALVE, CHECK: TYPE: NON RETURN; VALVE SIZE: 20 MM; DESIGN RATING: 16 BAR; TEMPERATURE RATING: -10 TO 120 DEG C; CONNECTION: SCREWED TO BSP TREADED FEMALE; BODY MATERIAL: BRONZE; FACE TO FACE LENGTH: 52 MM; OPERATED: SPRING; WATER TREATMENT PLANT, 2270 BRONZE, C/W RESILIENT SEAT, THREADED FEMALE, SUPPLIER TO SUPPLY WITH THE PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATES.","DATA NOT AVAILABLE","CHECK; NON RETURN","20 MM","BRONZE","16 BAR",null,"SCREWED TO BSP TREADED FEMALE","52 MM",null,"SPRING",null,"-10 TO 120 DEG C",{"$nulls":3},"PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATES; CERTIFICATES"]
["Palmiet Pumped Storage Scheme",783420,"VALVE, GATE: VALVE SIZE: 250 MM; TYPE: GATE VALVE; DESIGN PRESSURE: 10 BAR; DESIGN TEMPERATURE: -29 TO 420 DEG C; CONNECTION: FLANGE DRILLED TO JIS 10K50; FACE TO FACE LENGTH: 332 MM; BODY MATERIAL: WCB; TRIM: TRIM 8; OPERATED: MANUAL; DUPLEX INLET AND OUTLET VALVE, DRILLED TO JIS10K250, RISING STEM, BA-OOP, WORN&WHEEL GEAR, STEM HANDWHEEL WITH POSITION INDICATOR, PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATE ON DELIVERY.","DATA NOT AVAILABLE","GATE; DRILLED TO JIS10K250, RISING STEM, BA-OOP, WORN&WHEEL GEAR, STEM HANDWHEEL WITH POSITION INDICATOR, PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATE ON DELIVERY; GATE VALVE","250 MM","WCB","10 BAR","TRIM 8","FLANGE DRILLED TO JIS 10K50","332 MM",null,"MANUAL",null,"-29 TO 420 DEG C",{"$nulls":3},"PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATE ON DELIVERY; CERTIFICATE ON DELIVERY"]
["Palmiet Pumped Storage Scheme",692548,"VALVE, CHECK: TYPE: SWING DISK NRV; VALVE SIZE: 1 IN; DESIGN RATING: 300 LB; TEMPERATURE RATING: 38 DEG C; CONNECTION: FNPT; BODY MATERIAL: SS FORGED STEEL; FACE TO FACE LENGTH: 216 MM; OPERATED: AUTO; STYLE: THD BONNET; TRIM: BRASS; SOFTGOODS: SEAL NBR, BACK UP RING PTFE; APPLICATION: PREVENT BACKFLOW; SPECIFICATION: LB (ASA); GRADE: ANSI-300; FLANGED ENDS TO ANSI-300 LB (ASA)","DATA NOT AVAILABLE","CHECK; SWING DISK NRV","1 IN","SS FORGED STEEL","300 LB","BRASS","FNPT","216 MM",null,"AUTO","PREVENT BACKFLOW","38 DEG C",null,null,"SEAL NBR, BACK UP RING PTFE"]
["Palmiet Pumped Storage Scheme",783648,"VALVE, GLOBE: VALVE SIZE: 25 MM; DESIGN PRESSURE: 10 BAR; DESIGN TEMPERATURE: 120 DEG C; FACE TO FACE LENGTH: 127 MM; OPERATED: MANUAL; CONNECTION: FLANGED DRILLED TO JIS 10K; BODY MATERIAL: WCB; TRIM: 8; STEM DESIGN: NON RISING STEM; 10K25 ,UGB OIL COOLER ISOLATING VALVE, PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY","DATA NOT AVAILABLE","GLOBE; PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY","25 MM","WCB","10 BAR","8; NON RISING STEM","FLANGED DRILLED TO JIS 10K","127 MM",null,"MANUAL",null,"120 DEG C",{"$nulls":3},"PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY; CERTIFICATES TO BE SUPPLIED UPON DELIVERY"]
["Palmiet Pumped Storage Scheme",783662,"VALVE, CHECK: TYPE: WAFER; VALVE SIZE: 150 MM; DESIGN RATING: 16 BAR; TEMPERATURE RATING: 5 to 40 DEG C; CONNECTION: NO FLANGE; BODY MATERIAL: CAST IRON; FACE TO FACE LENGTH: 76 MM; OPERATED: AUTOMATIC; STYLE: WAFER; TRIM: COPON COATED; SOFTGOODS: EPDM; MANUF P/N: FIG 316; SEEPAGE PUMP DISCHARGE VALVE, WAFER TYPE, EPDM DIAPHRAGM, COPEN LINED, RIENZI, SUPPLIER TO SUPPLY WITH THE PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATES.","DATA NOT AVAILABLE","CHECK; WAFER TYPE, EPDM DIAPHRAGM, COPEN LINED, RIENZI, SUPPLIER TO SUPPLY WITH THE PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATES; WAFER","150 MM","CAST IRON","16 BAR","COPON COATED","NO FLANGE","76 MM",null,"AUTOMATIC",null,"5 to 40 DEG C","FIG 316",null,"EPDM","PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATES; CERTIFICATES"]
["Palmiet Pumped Storage Scheme",783651,"VALVE, GLOBE: VALVE SIZE: 50 MM; DESIGN PRESSURE: 16 BAR; DESIGN TEMPERATURE: -120 to 200 DEG C; FACE TO FACE LENGTH: 225 MM; OPERATED: MANUAL; CONNECTION: FLANGED DRUILLED TO JIS 10K RAISED FACE; BODY MATERIAL: GG25; TRIM: 2; SPECIFICATION: NON RISING STEM; PT UPPER TANK , BODY AND SEAL PRESSURE TEST CERTIFICATES AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY","DATA NOT AVAILABLE","GLOBE","50 MM","GG25","16 BAR",2,"FLANGED DRUILLED TO JIS 10K RAISED FACE","225 MM",null,"MANUAL",null,"-120 to 200 DEG C",{"$nulls":3},"PRESSURE TEST CERTIFICATES AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY; CERTIFICATES AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY"]
["Palmiet Pumped Storage Scheme",783429,"VALVE, CHECK: TYPE: SWING; VALVE SIZE: 50 MM; DESIGN RATING: 76 BAR; TEMPERATURE RATING: 538 DEG C; CONNECTION: FLANGED , DRILLED TO EN1092-1 PN 40; BODY MATERIAL: 316 SS; FACE TO FACE LENGTH: 265 MM; OPERATED: PRESSURE OPEN/CLOSE; SPECIFICATION: CLASS 300; NEWAY , BS1868,LABYRINTH COOLING WATER SYSTEM , PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY.","DATA NOT AVAILABLE","CHECK; SWING","50 MM","316 SS","76 BAR",null,"FLANGED , DRILLED TO EN1092-1 PN 40","265 MM",null,"PRESSURE OPEN/CLOSE",null,"538 DEG C",{"$nulls":3},"PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY; CERTIFICATES TO BE SUPPLIED UPON DELIVERY"]
["Palmiet Pumped Storage Scheme",783504,"VALVE, GLOBE: VALVE SIZE: 100 MM; DESIGN PRESSURE: 16 BAR; DESIGN TEMPERATURE: 400 DEG; FACE TO FACE LENGTH: 230 MM; OPERATED: MANUAL; CONNECTION: FLANGED DRILLED TO BS4504 T16; BODY MATERIAL: STAINLESS STEEL; TRIM: STAINLESS STEEL; MANUF P/N: GMK-GV-DN100-PN16-F2-WCB; TGB COOLER CW INLET & OUTLET VALVE, METAL VALVES(GMK), DIN3356, PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATES TO BE SUPPLIED ON DELIVERY.","GMK","GLOBE; METAL VALVES(GMK), DIN3356, PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATES TO BE SUPPLIED ON DELIVERY","100 MM","STAINLESS STEEL","16 BAR","STAINLESS STEEL","FLANGED DRILLED TO BS4504 T16","230 MM",null,"MANUAL",null,"400 DEG","GMK-GV-DN100-PN16-F2-WCB",null,null,"PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATES TO BE SUPPLIED ON DELIVERY; CERTIFICATES TO BE SUPPLIED ON DELIVERY"]
["Palmiet Pumped Storage Scheme",783652,"VALVE, GATE: VALVE SIZE: 250 MM; TYPE: SOLID WEDGE; DESIGN PRESSURE: 10 BAR; DESIGN TEMPERATURE: 120 DEG C; CONNECTION: FLANGED DRILLED TO JIS 10K; FACE TO FACE LENGTH: 329 MM; BODY MATERIAL: WCB; TRIM: 8; OPERATED: MANUAL - HANDWHEEL; STEM DESIGN: RISING STEM; APPLICATION: GEN COOLER CW ISOLATE; SPECIFICATION: 10K250; MANUF P/N: BA-00P; LIMITORQUE , HANDWHEEL ACTUATOR WORM AND GEAR SYSTEM.PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY","DATA NOT AVAILABLE","GATE; SOLID WEDGE","250 MM","WCB","10 BAR","8; RISING STEM","FLANGED DRILLED TO JIS 10K","329 MM",null,"MANUAL - HANDWHEEL","GEN COOLER CW ISOLATE","120 DEG C","BA-00P",null,null,"PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY; CERTIFICATES TO BE SUPPLIED UPON DELIVERY"]
["Palmiet Pumped Storage Scheme",783647,"VALVE, GATE: VALVE SIZE: 80 MM; TYPE: SOLID WEDGE; DESIGN PRESSURE: 10 BAR; DESIGN TEMPERATURE: 120 DEG C; CONNECTION: FLANGED DRILLED TO JIS 10K; FACE TO FACE LENGTH: 200 MM; BODY MATERIAL: WCB; TRIM: 8; OPERATED: HANDWHEEL MANUAL OPERATED; STEM DESIGN: RISING STEM; UPPER GUIDE BEARING OIL ISOLATE,PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY","DATA NOT AVAILABLE","GATE; SOLID WEDGE","80 MM","WCB","10 BAR","8; RISING STEM","FLANGED DRILLED TO JIS 10K","200 MM",null,"HANDWHEEL MANUAL OPERATED",null,"120 DEG C",{"$nulls":3},"PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY; CERTIFICATES TO BE SUPPLIED UPON DELIVERY"]
["Palmiet Pumped Storage Scheme",784003,"VALVE, RELIEF: VALVE SIZE: 1 IN; SET PRESSURE: 600 KPA G; TEMPERATURE RATING: -20 TO -260 DEG C; CONNECTION: THREADED 1G MALE INLET 1G FEMALE OUTLET; BODY MATERIAL: BRASS; TRIM: STAINLESS/BRONZE; FACE TO FACE LENGTH: 44 MM; OPERATED: PRESSURE SPRING RELEASE; APPLICATION: FIRE PUMP RELIEF VALVES; STYLE: RIGHT ANGLED SAFETY VALVE; TYPE 485 BAILEY BIRKETT, PRESSURE SET TO 600KPA , PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY.","DATA NOT AVAILABLE","RELIEF","1 IN","BRASS","600 KPA G","STAINLESS/BRONZE","THREADED 1G MALE INLET 1G FEMALE OUTLET","44 MM",null,"PRESSURE SPRING RELEASE","FIRE PUMP RELIEF VALVES","-20 TO -260 DEG C",{"$nulls":3},"PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY; CERTIFICATES TO BE SUPPLIED UPON DELIVERY"]
["Palmiet Pumped Storage Scheme",784000,"VALVE, BUTTERFLY: TYPE: WAFER; VALVE SIZE: 6 IN; DESIGN RATING: 20.7 BAR; TEMPERATURE RATING: 100 DEG C; CONNECTION: CLAMPED; BODY MATERIAL: DUCTILE IRON; FACE TO FACE LENGTH: 61 MM; OPERATED: HANDWHEEL AND GEAR ACTUATED; TRIM: NYLON-RILSON FIRE POWDERS (PA11)BLACK; SOFTGOODS: EPDM ENCAPSULATED; APPLICATION: FIRE WATER SYSTEM TEST VALVE; SPECIAL FEATURES: UL & FM APPROVED CE CERTIFIED; MANUF P/N: BFV 300; TYCO","Tyco Fire Products (Johnson Controls)","BUTTERFLY; WAFER","6 IN","DUCTILE IRON","20.7 BAR","NYLON-RILSON FIRE POWDERS (PA11)BLACK","CLAMPED","61 MM",null,"HANDWHEEL AND GEAR ACTUATED","FIRE WATER SYSTEM TEST VALVE","100 DEG C","BFV 300",null,"EPDM ENCAPSULATED"]
["Palmiet Pumped Storage Scheme",784005,"VALVE, GATE: VALVE SIZE: 200 MM; TYPE: SOLID WEDGE; DESIGN PRESSURE: 16 BAR; DESIGN TEMPERATURE: 5 TO 40 DEG C; CONNECTION: FLANGED DRILLED TO BS4504 T16; FACE TO FACE LENGTH: 317 MM; BODY MATERIAL: SPHEROIDAL GRAPHITE IRON; TRIM: 8; OPERATED: MANUAL HANDWHEEL; APPLICATION: FIRE RESERVOIR INLET; SPECIAL FEATURES: RESILIENT SEAT VALVE; PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY","DATA NOT AVAILABLE","GATE; SOLID WEDGE","200 MM","SPHEROIDAL GRAPHITE IRON","16 BAR",8,"FLANGED DRILLED TO BS4504 T16","317 MM",null,"MANUAL HANDWHEEL","FIRE RESERVOIR INLET","5 TO 40 DEG C",null,null,"E","PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY; CERTIFICATES TO BE SUPPLIED UPON DELIVERY"]
["Palmiet Pumped Storage Scheme",784002,"VALVE, GATE: VALVE SIZE: 250 MM; TYPE: SOLID WEDGE; DESIGN PRESSURE: 16 BAR; DESIGN TEMPERATURE: 5 TO 40 DEG C; CONNECTION: FLANGED DRILLED TO BS4504 T16; FACE TO FACE LENGTH: 380 MM; BODY MATERIAL: SPHEROIDAL GRAPHITE IRON; TRIM: 8; OPERATED: MANUAL HANDWHEEL; APPLICATION: FIRE PUMP INLET AND OUTLET; SPECIAL FEATURES: RESILIENT SEAT VALVE; PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY,AINSWORTH","Ainsworth","GATE; SOLID WEDGE","250 MM","SPHEROIDAL GRAPHITE IRON","16 BAR",8,"FLANGED DRILLED TO BS4504 T16","380 MM",null,"MANUAL HANDWHEEL","FIRE PUMP INLET AND OUTLET","5 TO 40 DEG C",null,null,"E","PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY,AINSWORTH; CERTIFICATES TO BE SUPPLIED UPON DELIVERY,AINSWORTH"]
["Palmiet Pumped Storage Scheme",784001,"VALVE, GATE: VALVE SIZE: 2 IN; TYPE: SOLID WEDGE; DESIGN PRESSURE: 20 BAR; DESIGN TEMPERATURE: -20 to 200 DEG C; CONNECTION: THREADED FEMALE BOTH ENDS BSPP; FACE TO FACE LENGTH: 74 MM; BODY MATERIAL: BRASS ALLOY; TRIM: BRASS; OPERATED: HAND WHEEL OPERATED; APPLICATION: JOCKEY FIRE PUMP ISOLATING VALVE; PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY","DLM","GATE; SOLID WEDGE","2 IN","BRASS ALLOY","20 BAR","BRASS","THREADED FEMALE BOTH ENDS BSPP","74 MM",null,"HAND WHEEL OPERATED","JOCKEY FIRE PUMP ISOLATING VALVE","-20 to 200 DEG C",{"$nulls":3},"PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY; CERTIFICATES TO BE SUPPLIED UPON DELIVERY"]
["Palmiet Pumped Storage Scheme",784004,"VALVE, CHECK: TYPE: SPRING; VALVE SIZE: 50 MM; DESIGN RATING: 18 BAR; TEMPERATURE RATING: -20 to 200 DEG C; CONNECTION: THREADED BSPP FEMALE BOTH ENDS; BODY MATERIAL: BRASS ALLOY; FACE TO FACE LENGTH: 101 MM; OPERATED: PRESSURE OPERATED; APPLICATION: JOCKEY FIRE PUMP NRV; MANUF P/N: ITAP 21-2; EUROPA , PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY","Europa / ITAP","CHECK; SPRING","50 MM","BRASS ALLOY","18 BAR",null,"THREADED BSPP FEMALE BOTH ENDS","101 MM",null,"PRESSURE OPERATED","JOCKEY FIRE PUMP NRV","-20 to 200 DEG C","ITAP 21-2",null,null,"PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY; CERTIFICATES TO BE SUPPLIED UPON DELIVERY"]
["Ingula Pumped Storage Scheme",41833,"VALVE: TYPE: COMPRESSOR; VALVE SIZE: 175 MM; OPERATED: PRESSURE; BODY MATERIAL: STL; TRIM: DISC SS; 2ND STAGE CONCENTRIC","SAUER COMPRESSOR","COMPRESSOR","175 MM","STL","27BAR","DISC SS","N/A","N/A","N/A","PRESSURE","COMPRESSED AIR","50 DEG C"]
["Ingula Pumped Storage Scheme",62540,"VALVE, SOLENOID: POTENTIAL: 220 V; SUPPL P/N: S2155",null,"SOLENOID",{"$nulls":10},"S2155","220 V"]
["Ingula Pumped Storage Scheme",63385,"SEAT: TYPE: DISC SAFETY VALVE; DIMENSIONS: SQ 0.514 IN; MATERIAL: 1.4122 DIN X 35CRMO17; SUPPL P/N: 018109610; 601267620; MODEL NO: VSE2.40.25.A.50.I.22.123; USED ON SEMPELL; POSITION CODE RL01S010, RL02S009, RL03S008","Sempell","DISC SAFETY VALVE","SQ 0,51410 IN","1.4122 DIN X 35CRMO17","P/N: 018109610; 601267620","SEAT","NO END CONNECTION","N/A","N/A","PASSIVE SEALING","SEMPELL","400-450°C","018109610; VSE2.40.25.A.50.I.22.123",null,"TYPE: DISC SAFETY VALVE"]
["Ingula Pumped Storage Scheme",65928,"BALL VLV:16 MM;STL","PISTER","Ball","16MM","STAINLESS STEEL","PN400","BALL, SEATS, STEM,SEALS","MALE CONNECTION","COMPACT, NON STANDARD DIMENSION","N/A","MANUAL","OIL","180°C"]
["Ingula Pumped Storage Scheme",72645,"VALVE: TYPE: HYDRAULIC; VALVE SIZE: 3/4 IN","PISTER/UFIXED/HYDEC","HYDRAULIC","3/4 IN","STAINLESS STEEL","PN315","STAINLESS STEEL, ","THREADED","≈ 70 – 120 mm","N/A","MANUALLY","HYDRAULIC OIL","–20°C to +80°C"]
["Ingula Pumped Storage Scheme",619974,"VALVE, RELIEF: VALVE SIZE: 1/2 IN; SET PRESSURE: 1.5 MPA; TEMPERATURE RATING: 120 DEG C; CONNECTION: BSP SCREW; BODY MATERIAL: STEEL; TRIM: STEEL; FACE TO FACE LENGTH: T-TYPE; OPERATED: PRESSURE; APPLICATION: PRESSURE REDUCER; DESIGN RATING: 1.5 MPA; PRESSURE RANGE: 1.3-1.5 MPA; REFERENCE NO: ESV-903M","REXROTH","RELIEF","1/2 IN","STEEL","1.5 MPA; 1.3-1.5 MPA","STEEL","BSP SCREW","T-TYPE","N/A","PRESSURE","PRESSURE REDUCER","120 DEG C","ESV-903M"]
["Ingula Pumped Storage Scheme",619983,"VALVE, BALL: VALVE SIZE: 50 MM; DESIGN RATING: 10 KPA; TEMPERATURE RATING: JIS10K; CONNECTION: FLANGED; BODY MATERIAL: SCPH2/304; FACE TO FACE LENGTH: 175 MM; OPERATED: LEVER; STYLE: DIRECTIONAL; TRIM: STL; SOFTGOODS: PTFE; APPLICATION: UPPER OIL COOLER; TYPE: ISOLATING","PARKER, PISTER, KLINGER MZANSI","BALL; ISOLATING","50 MM","SCPH2/304","10 KPA","STL","FLANGED","175 MM","120 MM","LEVER","UPPER OIL COOLER","JIS10K",null,null,"PTFE"]
["Ingula Pumped Storage Scheme",620183,"VALVE, GLOBE: VALVE SIZE: 1/2 IN; DESIGN PRESSURE: 2.0 MPA; DESIGN TEMPERATURE: <100 DEG C; FACE TO FACE LENGTH: 150 MM; OPERATED: HANDWHEEL; CONNECTION: FLANGED; BODY MATERIAL: F304; TRIM: SS GR 304/STL; GRADE: ASTM A182 F304; SOFTGOODS: NEOPRENE; STEM DESIGN: RISING SPINDLE; STYLE: DIRECTIONAL; APPLICATION: DRAIN AIR/OIL COOLER; SPECIFICATION: ISO9001; TYPE: SHUT OFF; DESIGN RATING: JIS 20K; S AND S VALVE","VALVE FOR AFRICA ,SUPERPUMP, KLINGER MZANSI","GLOBE; SHUT OFF","1/2 IN","F304","JIS 20K; 2.0 MPA","SS GR 304/STL; RISING SPINDLE","FLANGED","150 MM","70 MM","HANDWHEEL","DRAIN AIR/OIL COOLER","<100 DEG C",null,null,"NEOPRENE"]
["Ingula Pumped Storage Scheme",620391,"VALVE, GATE: VALVE SIZE: 250 MM; TYPE: ISOLATING; DESIGN PRESSURE: 2-2.8 MPA; DESIGN TEMPERATURE: 220-350 DEG C; CONNECTION: FLANGE; FACE TO FACE LENGTH: 455 MM; BODY MATERIAL: STAINLESS STEEL; TRIM: HF; OPERATED: ACTUATOR; STEM DESIGN: NON RISING; STYLE: 1 WAY; TEMPERATURE RATING: 20 K; PORT TYPE: STANDARD; APPLICATION: TURBINE; SPECIFICATION: ISO 9001; SPECIAL FEATURES: NONE; GRADE: 304; DESIGN RATING: JIS 20K","KITZ Corporation , Velan Inc. , Kubota Corporation","GATE; ISOLATING; STANDARD","250 MM","STAINLESS STEEL","JIS 20K; 2-2.8 MPA","HF; NON RISING","FLANGE","455 MM","Pitch Circle Diameter (PCD): 380 mm (The center-to-center diameter of the bolt circle)Number of Bolt Holes: 12 holesBolt Hole Diameter: 27 mm (Designed to fit metric M24 flange bolts)","ACTUATOR","TURBINE","20 K; 220-350 DEG C"]
["Ingula Pumped Storage Scheme",620405,"VALVE, BALL: VALVE SIZE: 200 MM; DESIGN RATING: JIS 10 K; TEMPERATURE RATING: 10 K; CONNECTION: FLANGE; BODY MATERIAL: SS GR 304; FACE TO FACE LENGTH: 455 MM; OPERATED: ACTUATOR, HANDWHEEL; STYLE: 1 WAY; SOFTGOODS: PTFE; APPLICATION: GENERATOR; TYPE: ISOLATING; .","PARKER, HYDEC, VALVES FOR AFRICA","BALL; ISOLATING","200 MM","SS GR 304","JIS 10 K","BALL, STEM, GLAND PACKING FOLLOWER (STAINLESS STEEL), SEALS, PACKING (PTFE)","FLANGE","455 MM","75 MM","ACTUATOR, HANDWHEEL","GENERATOR","10 K",null,null,"PTFE"]
["Ingula Pumped Storage Scheme",620407,"VALVE, GLOBE: VALVE SIZE: 50 MM; FACE TO FACE LENGTH: 200 MM; OPERATED: HANDWHEEL; CONNECTION: FLANGE; BODY MATERIAL: SCS13; TRIM: SS GR 304; STEM DESIGN: RISING; STYLE: 1 WAY; APPLICATION: DRAIN; TYPE: ISOLATING; DESIGN RATING: JIS 20K; TEMPERATURE RATING: 20K","PAKER, SUPERPUMP , HYDRAULICS, PISTER","GLOBE; ISOLATING","50 MM","SCS13","JIS 20K","SS GR 304; RISING","FLANGE","200 MM","120 MM","HANDWHEEL","DRAIN","20K"]
["Ingula Pumped Storage Scheme",620408,"VALVE, GLOBE: VALVE SIZE: 2 IN; FACE TO FACE LENGTH: 200 MM; OPERATED: HANDWHEEL; CONNECTION: FLANGE; BODY MATERIAL: A105; TRIM: 13CR; STEM DESIGN: RISING; STYLE: 1 WAY; APPLICATION: DRAIN; TYPE: ISOLATING; DESIGN RATING: JIS 10K; TEMPERATURE RATING: 840 DEG F","PAKER, SUPERPUMP , HYDRAULICS, PISTER","GLOBE; ISOLATING","2 IN","A105","JIS 10K","13CR; RISING","FLANGE","200 MM","120 MM","HANDWHEEL","DRAIN","840 DEG F"]
["Ingula Pumped Storage Scheme",628662,"VALVE: TYPE: SAFETY; VALVE SIZE: 4 IN; DESIGN RATING: 53 BAR; TEMPERATURE RATING: 538 DEG C; CONNECTION: FLANGE; OPERATED: PRESSURE, SPRING, 0-35 LB; BODY MATERIAL: BS 1504-240; STYLE: ANGLE PATTERN; TRIM: PT; OEM P/N: 4\"707 SD; DRAWING NO: F5217/5 REV 0; .","LESER,REXROTH","SAFETY","4 IN","BS 1504-240","53 BAR","PT","FLANGE","320 - 400 MM","190 MM","PRESSURE, SPRING, 0-35 LB","STEAM","538 DEG C","4\"707 SD; F5217/5 REV 0"]
["Ingula Pumped Storage Scheme",628694,"VALVE, BALL: VALVE SIZE: 50 MM; DESIGN RATING: 63 BAR; TEMPERATURE RATING: 200 DEG C; CONNECTION: FEMALE THD; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 140 MM; OPERATED: HAND; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: PTFE; SPECIFICATION: JT97AN; PORT TYPE: BALL; APPLICATION: VARIOUS; GRADE: 1.4408; TYPE: ISOLATING","PARKER, PISTER, KLINGER MZANSI","BALL; ISOLATING","50 MM","STAINLESS STEEL","63 BAR","STAINLESS STEEL","FEMALE THD","140 MM","N/A","HAND","VARIOUS","200 DEG C",null,null,"PTFE"]
["Ingula Pumped Storage Scheme",628697,"VALVE, RELIEF: VALVE SIZE: 3/4 IN; SET PRESSURE: 47.2 BAR; TEMPERATURE RATING: -10 TO 100 DEG C; CONNECTION: THREADED FEMALE; BODY MATERIAL: BRASS; TRIM: BRASS; FACE TO FACE LENGTH: 118 MM; OPERATED: PRESSURE; ORIFICE SIZE: 10 MM; SPECIFICATION: ISO 4126-1; APPLICATION: VARIOUS; STYLE: 1 WAY; SOFTGOODS: BRASS; DESIGN RATING: 150 BAR; PRESSURE RANGE: 42-25 BAR; MANUF P/N: H10N11787","REXROTH","RELIEF","3/4 IN; 10 MM","BRASS","150 BAR; 42-25 BAR; 47.2 BAR","BRASS","THREADED FEMALE","118 MM","N/A","PRESSURE","VARIOUS","-10 TO 100 DEG C","H10N11787",null,"BRASS"]
["Ingula Pumped Storage Scheme",637382,"VALVE: TYPE: CONCENTRIC; VALVE SIZE: OD 225 X THK 30 MM; DESIGN RATING: 380 BAR; TEMPERATURE RATING: -28 TO 425 DEG C; CONNECTION: SEAT; OPERATED: MECHANICAL; BODY MATERIAL: STAINLESS STEEL; STYLE: LEAF; MANUF P/N: 37134; MODEL NO: WP6310; FOR USE ON JP SAUER AND SOHN COMPRESSOR","SAUER COMPRESSOR","CONCENTRIC","OD 225 X THK 30 MM","STAINLESS STEEL","380 BAR","STAINLESS STEEL","SEAT","N/A","N/A","MECHANICAL","JP SAUER AND SOHN COMPRESSOR","-28 TO 425 DEG C","37134; WP6310"]
["Ingula Pumped Storage Scheme",637420,"VALVE, BALL: VALVE SIZE: DN 50; DESIGN RATING: PN100; TEMPERATURE RATING: 0-30 DEG C; CONNECTION: FLANGE; BODY MATERIAL: 1.4571; OPERATED: LEVER; SPECIFICATION: SAE; DIN; ANSI; ISO; TYPE: HYDRAULIC; REFERENCE NO: 190-050-138","PARKER, PISTER, KLINGER MZANSI","BALL; HYDRAULIC","DN 50",1.4571,"PN100","STAINLESS STEEL BALL AND BALL WITH PTFE SEATS AND PACKING, REINFORCED SEALING ELEMENTS SUITABLE FOR HIGH- PRESSURE HYDRAULIC SERVICE","FLANGE","150 MM","125 MM","LEVER","HYDRAULIC FLUID, WATER BASED FLUID, LIGHT GASE AND CHEMICALS","0-30 DEG C","190-050-138"]
["Ingula Pumped Storage Scheme",637421,"VALVE, BALL: VALVE SIZE: DN 100; DESIGN RATING: PN100; TEMPERATURE RATING: -10 TO 50 DEG C; CONNECTION: FLANGE; BODY MATERIAL: 1.4571; OPERATED: LEVER; SPECIFICATION: SAE; DIN; ANSI; ISO; TYPE: PNEUMATIC; REFERENCE NO: 190-100-202; .","PARKER, PISTER, KLINGER MZANSI, VOITH","BALL; PNEUMATIC","DN 100",1.4571,"PN100","STAINLESS STEEL","FLANGE","≈ 230 mm","190 MM","LEVER","HYDRAULIC AND PNEUMATIC SYSTEMS, WATER SERVICES, GASES, LIGHT CHEMICAL FLUIDS","-10 TO 50 DEG C","190-100-202"]
["Ingula Pumped Storage Scheme",637560,"VALVE, RELIEF: VALVE SIZE: 1 IN; SET PRESSURE: 88 BAR; TEMPERATURE RATING: 0-50 DEG C; CONNECTION: G1 IN-BSPP; BODY MATERIAL: STAINLESS STEEL; TRIM: STAINLESS STEEL; FACE TO FACE LENGTH: L SHAPE; OPERATED: AIR; ORIFICE SIZE: 1 IN; SPECIFICATION: GL1238640; APPLICATION: COMPRESSOR; GRADE: 316; STYLE: 1 WAY; SOFTGOODS: STAINLESS STEEL; DESIGN RATING: 88 BAR G; PRESSURE RANGE: IN PN 250; OUT PN 40; MANUF P/N: M33H03X00V56V66J23H01","REXROTH,VOITH","RELIEF","1 IN","STAINLESS STEEL","88 BAR G; IN PN 250; 88 BAR","STAINLESS STEEL","G1 IN-BSPP","L SHAPE","N/A","AIR","COMPRESSOR","0-50 DEG C","M33H03X00V56V66J23H01",null,"STAINLESS STEEL"]
["Ingula Pumped Storage Scheme",637562,"VALVE, RELIEF: VALVE SIZE: 1/2 IN; SET PRESSURE: 3 BAR; TEMPERATURE RATING: 0-20 DEG C; CONNECTION: THD 1/2 IN; BODY MATERIAL: STAINLESS STEEL; TRIM: STAINLESS STEEL; FACE TO FACE LENGTH: L SHAPE; OPERATED: AIR; ORIFICE SIZE: 1 IN; SPECIFICATION: 14/980; APPLICATION: COMPRESSOR; GRADE: 316; STYLE: 1 WAY; SOFTGOODS: STAINLESS STEEL; DESIGN RATING: 3 BAR; PRESSURE RANGE: IN PN 250; OUT PN 160; MANUF P/N: M33H03X00V54V65; .","REXROTH,VOITH","RELIEF","1/2 IN; 1 IN","STAINLESS STEEL","3 BAR; IN PN 250","STAINLESS STEEL","THD 1/2 IN","L SHAPE","N/A","AIR","COMPRESSOR","0-20 DEG C","M33H03X00V54V65",null,"STAINLESS STEEL"]
["Ingula Pumped Storage Scheme",638401,"VALVE, BALL: VALVE SIZE: 1/2 IN; DESIGN RATING: PN30; TEMPERATURE RATING: 0-200 DEG C; CONNECTION: FEMALE THD; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 59 MM; OPERATED: LEVER; STYLE: 1 WAY; TRIM: BRASS; SOFTGOODS: NYLON; APPLICATION: FIRE SYSTEM; GRADE: 316; TYPE: LOCKABLE; MANUF P/N: 1610LD210","PISTER, PARKER,HYDEC","BALL; LOCKABLE","1/2 IN","STAINLESS STEEL","PN30","BRASS","FEMALE THD","59 MM","N/A","LEVER","FIRE SYSTEM","0-200 DEG C","1610LD210",null,"NYLON"]
["Ingula Pumped Storage Scheme",638405,"VALVE, ANGLE: TYPE: SUPPLY; VALVE SIZE: 80 MM; DESIGN RATING: 50 BAR; TEMPERATURE RATING: 300 DEG C; CONNECTION: THD FEMALE; BODY MATERIAL: BRASS; FACE TO FACE LENGTH: RIGHT ANGLE; OPERATED: HANDWHEEL; STYLE: 1 WAY; TRIM: RUBBER/SS; SOFTGOODS: BRASS; APPLICATION: FIRE HYDRANT; REFERENCE NO: VA001; KRS FIRE.","Krs Fire","ANGLE; SUPPLY","80 MM","BRASS","50 BAR","RUBBER/SS","THD FEMALE","RIGHT ANGLE","N/A","HANDWHEEL","FIRE HYDRANT","300 DEG C","VA001",null,"BRASS"]
["Ingula Pumped Storage Scheme",642473,"VALVE: TYPE: DIRECTIONAL; VALVE SIZE: 8/4 MM; DESIGN RATING: 350 BAR; TEMPERATURE RATING: 52 DEG C; FACE TO FACE LENGTH: 49 MM; CONNECTION: BOLT BLOCK; OPERATED: PRESSURE; BODY MATERIAL: STEEL; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SPECIFICATION: ISO 4401-03; SOFTGOODS: NBR; SPECIAL FEATURES: NIL; MANUF P/N: WDMFA06-AB3-G220/MD-HF1-P1AB",null,"DIRECTIONAL","8/4 MM","STEEL","350 BAR","STAINLESS STEEL","BOLT BLOCK","49 MM",null,"PRESSURE",null,"52 DEG C","WDMFA06-AB3-G220/MD-HF1-P1AB",null,"NBR"]
["Ingula Pumped Storage Scheme",643976,"VALVE, BALL: VALVE SIZE: DN 50; DESIGN RATING: PN200; TEMPERATURE RATING: 180 DEG C; CONNECTION: THD; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 140 MM; OPERATED: LEVER; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: PTFE; SPECIFICATION: ISO 9001; PORT TYPE: FULL BORE; APPLICATION: VARIOUS; GRADE: 1.4408; TYPE: LOCKABLE; BODY SHAPE: SQUARE","PARKER, PISTER, KLINGER MZANSI","BALL; FULL BORE; LOCKABLE","DN 50","STAINLESS STEEL","PN200","STAINLESS STEEL","THD","140 MM","N/A","LEVER","VARIOUS","180 DEG C",null,null,"PTFE"]
["Ingula Pumped Storage Scheme",643977,"VALVE, BALL: VALVE SIZE: 12 MM; DESIGN RATING: PN500; TEMPERATURE RATING: 180 DEG C; CONNECTION: 18L; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 115 MM; OPERATED: LEVER; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: NBR; SPECIFICATION: ISO 9001; PORT TYPE: FULL BORE; APPLICATION: VARIOUS; GRADE: 1.4571; TYPE: NON LOCKABLE; MANUF P/N: KH 18L-71X; BODY SHAPE: SQUARE","PISTER, PAKER, KLINGER MZANSI","BALL; FULL BORE; NON LOCKABLE","12 MM","STAINLESS STEEL","PN500","STAINLESS STEEL","18L","115 MM","N/A","LEVER","VARIOUS","180 DEG C","KH 18L-71X",null,"NBR"]
["Ingula Pumped Storage Scheme",643978,"VALVE, BALL: VALVE SIZE: 1/2 IN; DESIGN RATING: PN500; TEMPERATURE RATING: 180 DEG C; CONNECTION: THD; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 90 MM; OPERATED: LEVER; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: PTFE; SPECIFICATION: ISO 9001; PORT TYPE: FULL BORE; APPLICATION: VARIOUS; GRADE: 1.4423; TYPE: NON LOCKABLE; MANUF P/N: KH 1/2IN 71X; BODY SHAPE: SQUARE","PARKER, PISTER, KLINGER MZANSI","BALL; FULL BORE; NON LOCKABLE","1/2 IN","STAINLESS STEEL","PN500","STAINLESS STEEL","THD","90 MM","N/A","LEVER","VARIOUS","180 DEG C","KH 1/2IN 71X",null,"PTFE"]
["Ingula Pumped Storage Scheme",643979,"VALVE: TYPE: SHUT OFF; VALVE SIZE: DN 4; DESIGN RATING: PN250; TEMPERATURE RATING: 250 DEG C; FACE TO FACE LENGTH: 105 MM; CONNECTION: THD G1/2 IN; OPERATED: HANDWHEEL; BODY MATERIAL: BRASS; STYLE: 1 WAY; TRIM: BRASS; GRADE: C360; SPECIFICATION: ISO 9001; SOFTGOODS: BRASS; SPECIAL FEATURES: GAUGE/TRANSMITTER FITTING","BMG (BEARING MAN GROUP), AXIOM HYDRAULICS, HYTEC GROUP, VALUE AND AUTOMATION (PTY) LTD, SWAGELOK SOUTH AFRICA","SHUT OFF","DN 4","BRASS","PN250","BRASS","THD G1/2 IN","105 MM","N/A","HANDWHEEL","INSTRUMENTATION SERVICE-PRIMARILY COMPRESSED AIR OR NON- CORROSIVE FLUIDS USED FOR PRESSURE GAUGE AND TRANSMITTER ISOLATION","250 DEG C",null,null,"BRASS"]
["Ingula Pumped Storage Scheme",644949,"VALVE, RELIEF: VALVE SIZE: 10 MM; SET PRESSURE: 65 BAR; TEMPERATURE RATING: -30 TO 80 DEG C; CONNECTION: THREADED; BODY MATERIAL: STEEL; TRIM: METAL; FACE TO FACE LENGTH: 80 MM; OPERATED: PRESSURE; ORIFICE SIZE: 5 MM; SPECIFICATION: ISO 9001; APPLICATION: VARIOUS; GRADE: 913000149; STYLE: 1 WAY; SOFTGOODS: NBR; DESIGN RATING: 25-400 BAR; PRESSURE RANGE: 0-630 BAR; MANUF P/N: R901260712; MODEL NO: DBDS 10 G19/65E","REXROTH,VOITH","RELIEF","10 MM; 5 MM","STEEL","25-400 BAR; 0-630 BAR; 65 BAR","METAL","THREADED","80 MM","N/A","PRESSURE","VARIOUS","-30 TO 80 DEG C","R901260712; DBDS 10 G19/65E",null,"NBR"]
["Ingula Pumped Storage Scheme",644951,"VALVE, RELIEF: VALVE SIZE: 30 MM; SET PRESSURE: 130 BAR; TEMPERATURE RATING: -30 TO 80 DEG C; CONNECTION: SUBPLATE; BODY MATERIAL: STEEL; TRIM: METAL; FACE TO FACE LENGTH: 80 MM; OPERATED: PRESSURE; ORIFICE SIZE: 15 MM; SPECIFICATION: ISO 9001; APPLICATION: VARIOUS; GRADE: 913000149; STYLE: 1 WAY; SOFTGOODS: NBR; DESIGN RATING: 25-400 BAR; PRESSURE RANGE: 0-350 BAR; MANUF P/N: R901341824; MODEL NO: DBDS 30 G1A/130E","REXROTH,VOITH","RELIEF","30 MM; 15 MM","STEEL","25-400 BAR; 0-350 BAR; 130 BAR","METAL","SUBPLATE","80 MM","N/A","PRESSURE","VARIOUS","-30 TO 80 DEG C","R901341824; DBDS 30 G1A/130E",null,"NBR"]
["Ingula Pumped Storage Scheme",644953,"VALVE, RELIEF: VALVE SIZE: 20 MM; SET PRESSURE: 100 BAR; TEMPERATURE RATING: -30 TO 80 DEG C; CONNECTION: SUBPLATE; BODY MATERIAL: STEEL; TRIM: METAL; FACE TO FACE LENGTH: NIL; OPERATED: PRESSURE; ORIFICE SIZE: 10 MM; SPECIFICATION: ISO 9001; APPLICATION: VARIOUS; GRADE: 913000149; STYLE: 1 WAY; SOFTGOODS: NBR; DESIGN RATING: 25-400 BAR; PRESSURE RANGE: 10-350 BAR; MANUF P/N: R900597283; MODEL NO: DR 20-5-52/100YM","REXROTH, VOITH","RELIEF","20 MM; 10 MM","STEEL","25-400 BAR; 10-350 BAR; 100 BAR","METAL","SUBPLATE","NIL","N/A","PRESSURE","VARIOUS","-30 TO 80 DEG C","R900597283; DR 20-5-52/100YM",null,"NBR"]
["Ingula Pumped Storage Scheme",647409,"VALVE, SOLENOID: PIPE SIZE: 6 X 4 MM; STYLE: 3/2 WAY; POTENTIAL: 230 VAC; DESIGN RATING: 0-10 BAR; CONNECTION: G1/8 IN-BSPP; BODY MATERIAL: BRASS; OPERATED: AIR; ENCLOSURE RATING: IP65; MEDIUM: NATURAL GASES; FLUIDS; POWER: 8 W; ORIFICE SIZE: 2 MM; COIL: POLYAMIDE; SOFTGOODS: FKM; APPLICATION: FIRE DAMPER",null,"SOLENOID","6 X 4 MM; 2 MM","BRASS","0-10 BAR",null,"G1/8 IN-BSPP",null,null,"AIR","NATURAL GASES; FIRE DAMPER",null,null,"230 VAC; 8 W; POLYAMIDE; IP65","FKM"]
["Ingula Pumped Storage Scheme",648284,"VALVE: TYPE: EMERGENCY CLOSING; VALVE SIZE: 13 MM; DESIGN RATING: 350 BAR; TEMPERATURE RATING: 200 DEG C; FACE TO FACE LENGTH: FLAT; CONNECTION: THREADED; OPERATED: PRESSURE; BODY MATERIAL: STEEL; STYLE: 2 WAY; SPECIFICATION: ISO 9001; TURBINE GOVERNOR PUMP CONTROL; KKS: MFX20AA201/219","VOITH","EMERGENCY CLOSING","13 MM","STEEL","350 BAR","STAINLESS STEEL","THREADED","FLAT","N/A","PRESSURE","HIGH PRESSURE HYDRAULIC OIL, TURBINE GOVERNOR OIL SYSTEM","200 DEG C"]
["Ingula Pumped Storage Scheme",655228,"VALVE, RELIEF: VALVE SIZE: G1/2 IN; SET PRESSURE: 365 KPA; TEMPERATURE RATING: -10 TO 220 DEG C; CONNECTION: G1/2 IN; BODY MATERIAL: 1.4104 (430); TRIM: METAL; FACE TO FACE LENGTH: 46 MM; OPERATED: PRESSURE; ORIFICE SIZE: 10 MM; SPECIFICATION: DIN ISO 228-1; APPLICATION: VARIOUS; GRADE: 1.4104; STYLE: 1 WAY; SOFTGOODS: 1.4404; DESIGN RATING: PN160-400; PRESSURE RANGE: 180-365 BAR; MANUF P/N: 4373.2602; REFERENCE NO: D0 10-D/G 0.5 F 0.35; .","REXROTH","RELIEF","G1/2 IN; 10 MM","1.4104 (430)","PN160-400; 180-365 BAR; 365 KPA","METAL","G1/2 IN","46 MM","N/A","PRESSURE","VARIOUS","-10 TO 220 DEG C","4373.2602; D0 10-D/G 0.5 F 0.35",null,1.4404]
["Ingula Pumped Storage Scheme",692543,"VALVE: TYPE: NON RETURN; VALVE SIZE: 20 MM; TEMPERATURE RATING: -10 TO 100 DEG C; CONNECTION: 1/2 IN-BSP; OPERATED: AIR; BODY MATERIAL: STAINLESS STEEL; OEM P/N: 033930","SAUER COMPRESSOR","NON RETURN","20 MM","STAINLESS STEEL","PN16","STAINLESS STEEL ","1/2 IN-BSP","50 - 70 MM","N/A","AIR","COMPRESSED AIR","-10 TO 100 DEG C",33930]
["Ingula Pumped Storage Scheme",692898,"VALVE, SOLENOID: PIPE SIZE: 1/2 IN; STYLE: 1/1; POTENTIAL: 220 VDC; DESIGN RATING: 0-1.5 MPA; CONNECTION: BSPF; BODY MATERIAL: BRASS; OPERATED: SOLENOID; ENCLOSURE RATING: IP65; MEDIUM: AIR; ORIFICE SIZE: 3 MM; COIL: SINGLE; APPLICATION: MECHANICAL AIR BRAKE SYSTEM; OEM P/N: VS3P-4030-10G HMJ-X","VALVES FOR AFRIKA,SUPERPUMP, KLINGER MZANSI","SOLENOID","1/2 IN; 3 MM","BRASS","0-1.5 MPA","STAINLESS AND BRASS","BSPF","60 - 80 MM","PCD","SOLENOID","AIR; MECHANICAL AIR BRAKE SYSTEM","–10°C to +80°C","VS3P-4030-10G HMJ-X","220 VDC; SINGLE; IP65"]
["Ingula Pumped Storage Scheme",694573,"VALVE, SOLENOID: PIPE SIZE: 1 IN; STYLE: 1/1; POTENTIAL: 24 VDC; DESIGN RATING: 10 BAR; CONNECTION: FNPT; BODY MATERIAL: STAINLESS STEEL; OPERATED: COIL SOLENOID VALVE; ENCLOSURE RATING: IP65; MEDIUM: DIESEL; ORIFICE SIZE: 15-25 MM; COIL: SINGLE; SOFTGOODS: O RING; APPLICATION: DIESEL; MODEL NO 2W-160-15, BOTH VALVE PORT; SIZE 1 IN",null,"SOLENOID","1 IN; 15-25 MM","STAINLESS STEEL","10 BAR",null,"FNPT",null,null,"COIL SOLENOID VALVE","DIESEL",null,"2W-160-15, BOTH VALVE PORT","24 VDC; SINGLE; IP65","O RING"]
["Ingula Pumped Storage Scheme",715945,"VALVE, CHECK: TYPE: NON-RETURN; VALVE SIZE: 650 MM; DESIGN RATING: Y 0.35 AND VACUUM MPA; TEMPERATURE RATING: 200 DEG C; CONNECTION: BUTT-WELDED; BODY MATERIAL: STEEL ASTM A216-WCB; FACE TO FACE LENGTH: 1448 MM; OPERATED: AUTO; TRIM: STEEL; APPLICATION: CHECK VALVE LBS30AA501; SPECIFICATION: ANSI B16 34 CLASS 150; DRAWING NO: FB21EV650NFDA ITEM DEWRANCE; BLED STEAM CHECK VALVE, BODY: WBC, SEAT: CR13, DISK: CR18","Dewrance","CHECK; BODY; NON-RETURN","650 MM","STEEL ASTM A216-WCB","Y 0.35 AND VACUUM MPA","STEEL","BUTT-WELDED","1448 MM","N/A","AUTO","CHECK VALVE LBS30AA501","200 DEG C","FB21EV650NFDA ITEM DEWRANCE",null,"CR13, DISK: CR18"]
["Ingula Pumped Storage Scheme",726792,"VALVE, SOLENOID: PIPE SIZE: 28 MM; STYLE: COAXIAL 3/2 WAY DIRECT ACTING; POTENTIAL: 230 VAC; DESIGN RATING: 100 BAR; CONNECTION: G3/4 IN FEMALE; BODY MATERIAL: BRASS; OPERATED: SOLENOID; ENCLOSURE RATING: IP65; MEDIUM: AIR; POWER: 0.4 W; CURRENT: 0.15 A; ORIFICE SIZE: 15 MM; SOFTGOODS: NBR ORING; APPLICATION: DRAIN VALVE; MANUF P/N: 039599; STAGE 3 DRAIN VALVE","Coax","SOLENOID","28 MM; 15 MM","BRASS","100 BAR",null,"G3/4 IN FEMALE",null,null,"SOLENOID","AIR; DRAIN VALVE",null,39599,"230 VAC; 0.4 W; 0.15 A; IP65","NBR ORING"]
["Ingula Pumped Storage Scheme",628695,"VALVE, BALL: VALVE SIZE: 20 MM; DESIGN RATING: 40 BAR; TEMPERATURE RATING: 200 DEG C; CONNECTION: FLANGED; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 44 MM; OPERATED: HAND; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: PTFE; SPECIFICATION: K6HT; PORT TYPE: BALL; APPLICATION: VARIOUS; GRADE: 1.4408; TYPE: ISOLATING","KLINGER MZANSI, RHYNO VALVES,PARKER","BALL; ISOLATING","20 MM","STAINLESS STEEL","40 BAR","STAINLESS STEEL","FLANGED","44 MM",null,"HAND","VARIOUS","200 DEG C",null,null,"PTFE"]
["Ingula Pumped Storage Scheme",620405,"VALVE, BALL: VALVE SIZE: 200 MM; DESIGN RATING: JIS 10 K; TEMPERATURE RATING: 10 K; CONNECTION: FLANGE; BODY MATERIAL: SS GR 304; FACE TO FACE LENGTH: 455 MM; OPERATED: ACTUATOR, HANDWHEEL; STYLE: 1 WAY; SOFTGOODS: PTFE; APPLICATION: GENERATOR; TYPE: ISOLATING; .","PARKER, HYDEC, VALVES FOR AFRICA","BALL; ISOLATING","200 MM","SS GR 304","JIS 10 K","BALL, STEM, GLAND PACKING FOLLOWER (STAINLESS STEEL), SEALS, PACKING (PTFE)","FLANGE","455 MM","75 MM","ACTUATOR, HANDWHEEL","GENERATOR","10 K",null,null,"PTFE"]
["Ingula Pumped Storage Scheme",620406,"VALVE, BALL: VALVE SIZE: 200 MM; DESIGN RATING: JIS 10 K; TEMPERATURE RATING: 10 K; CONNECTION: FLANGE; BODY MATERIAL: SS GR 304; FACE TO FACE LENGTH: 455 MM; OPERATED: ACTUATOR, CHAIN; STYLE: 1 WAY; SOFTGOODS: PTFE; APPLICATION: GENERATOR; TYPE: ISOLATING","PARKER, PISTER, KLINGER MZANSI","BALL; ISOLATING","200 MM","SS GR 304","JIS 10 K","STAINLESS STEEL","FLANGE","455 MM","340 MM","ACTUATOR, CHAIN","GENERATOR","10 K",null,null,"PTFE"]
["Ingula Pumped Storage Scheme",692543,"VALVE: TYPE: NON RETURN; VALVE SIZE: 20 MM; TEMPERATURE RATING: -10 TO 100 DEG C; CONNECTION: 1/2 IN-BSP; OPERATED: AIR; BODY MATERIAL: STAINLESS STEEL; OEM P/N: 033930","SAUER COMPRESSOR","NON RETURN","20 MM","STAINLESS STEEL","PN16","STAINLESS STEEL ","1/2 IN-BSP","50 - 70 MM","N/A","AIR","COMPRESSED AIR","-10 TO 100 DEG C",33930]
["Ingula Pumped Storage Scheme",628696,"VALVE, BALL: VALVE SIZE: 1/2 IN; DESIGN RATING: 2000 KPA; TEMPERATURE RATING: 200 DEG C; CONNECTION: FEMALE THD; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 75 MM; OPERATED: HAND; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: PTFE; SPECIFICATION: 5BDB 5BEE; PORT TYPE: BALL; APPLICATION: VARIOUS; GRADE: 1.4408; TYPE: ISOLATING; MANUF P/N: CF8M","PARKER, PISTER, KLINGER MZANSI","BALL; ISOLATING","1/2 IN","STAINLESS STEEL","2000 KPA","STAINLESS STEEL","FEMALE THD","75 MM","N/A","HAND","VARIOUS","200 DEG C","CF8M",null,"PTFE"]
["Ingula Pumped Storage Scheme",643978,"VALVE, BALL: VALVE SIZE: 1/2 IN; DESIGN RATING: PN500; TEMPERATURE RATING: 180 DEG C; CONNECTION: THD; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 90 MM; OPERATED: LEVER; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: PTFE; SPECIFICATION: ISO 9001; PORT TYPE: FULL BORE; APPLICATION: VARIOUS; GRADE: 1.4423; TYPE: NON LOCKABLE; MANUF P/N: KH 1/2IN 71X; BODY SHAPE: SQUARE","PARKER, PISTER, KLINGER MZANSI","BALL; FULL BORE; NON LOCKABLE","1/2 IN","STAINLESS STEEL","PN500","STAINLESS STEEL","THD","90 MM","N/A","LEVER","VARIOUS","180 DEG C","KH 1/2IN 71X",null,"PTFE"]
["Ingula Pumped Storage Scheme",637420,"VALVE, BALL: VALVE SIZE: DN 50; DESIGN RATING: PN100; TEMPERATURE RATING: 0-30 DEG C; CONNECTION: FLANGE; BODY MATERIAL: 1.4571; OPERATED: LEVER; SPECIFICATION: SAE; DIN; ANSI; ISO; TYPE: HYDRAULIC; REFERENCE NO: 190-050-138","PARKER, PISTER, KLINGER MZANSI","BALL; HYDRAULIC","DN 50",1.4571,"PN100","STAINLESS STEEL BALL AND BALL WITH PTFE SEATS AND PACKING, REINFORCED SEALING ELEMENTS SUITABLE FOR HIGH- PRESSURE HYDRAULIC SERVICE","FLANGE","150 MM","125 MM","LEVER","HYDRAULIC FLUID, WATER BASED FLUID, LIGHT GASE AND CHEMICALS","0-30 DEG C","190-050-138"]
["Ingula Pumped Storage Scheme",643976,"VALVE, BALL: VALVE SIZE: DN 50; DESIGN RATING: PN200; TEMPERATURE RATING: 180 DEG C; CONNECTION: THD; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 140 MM; OPERATED: LEVER; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: PTFE; SPECIFICATION: ISO 9001; PORT TYPE: FULL BORE; APPLICATION: VARIOUS; GRADE: 1.4408; TYPE: LOCKABLE; BODY SHAPE: SQUARE","PARKER, PISTER, KLINGER MZANSI","BALL; FULL BORE; LOCKABLE","DN 50","STAINLESS STEEL","PN200","STAINLESS STEEL","THD","140 MM","N/A","LEVER","VARIOUS","180 DEG C",null,null,"PTFE"]
["Ingula Pumped Storage Scheme",657951,"VALVE, BALL: VALVE SIZE: DN 80; DESIGN RATING: PN100; TEMPERATURE RATING: 0-30 DEG C; CONNECTION: FLANGE; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 160 MM; OPERATED: ACTUATOR; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: PTFE; SPECIFICATION: ISO 9001; PORT TYPE: SCREW; APPLICATION: TURBINE; GRADE: 1.4301; TYPE: SHUT OFF; MODEL NO: FCKH; REFERENCE NO: 9423 107/15; PISTER","PARKER, PISTER, KLINGER MZANSI","BALL; SCREW; SHUT OFF","DN 80","STAINLESS STEEL","PN100","STAINLESS STEEL","FLANGE","160 MM","160 MM","ACTUATOR","TURBINE","0-30 DEG C","9423 107/15; FCKH",null,"PTFE"]
["Ingula Pumped Storage Scheme",657952,"VALVE, BALL: VALVE SIZE: DN 80; DESIGN RATING: PN100; TEMPERATURE RATING: 0-40 DEG C; CONNECTION: FLANGE; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 160 MM; OPERATED: ACTUATOR/LEVER; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: PTFE; SPECIFICATION: ISO 9001; PORT TYPE: SCREW; APPLICATION: TURBINE; GRADE: 1.4301; TYPE: SHUT OFF; MODEL NO: FCKH; REFERENCE NO: 9423 279/13; COMPLETE WITH EXTENSION; PISTER","PARKER, PISTER, VOITH","BALL; SCREW; SHUT OFF","DN 80","STAINLESS STEEL","PN100","STAINLESS STEEL","FLANGE","160 MM","160 MM","ACTUATOR/LEVER","TURBINE","0-40 DEG C","9423 279/13; FCKH",null,"PTFE"]
["Ingula Pumped Storage Scheme",657953,"VALVE, BALL: VALVE SIZE: DN 80; DESIGN RATING: PN100; TEMPERATURE RATING: 0-40 DEG C; CONNECTION: FLANGE; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 160 MM; OPERATED: ACTUATOR/LEVER; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: PTFE; SPECIFICATION: ISO 9001; PORT TYPE: SCREW; APPLICATION: TURBINE; GRADE: 1.4301; TYPE: SHUT OFF; MODEL NO: FCKH; REFERENCE NO: 9423 452/13; PISTER","PARKER, PISTER, VOITH","BALL; SCREW; SHUT OFF","DN 80","STAINLESS STEEL","PN100","STAINLESS STEEL","FLANGE","160 MM","160 MM","ACTUATOR/LEVER","TURBINE","0-40 DEG C","9423 452/13; FCKH",null,"PTFE"]
["Ingula Pumped Storage Scheme",628693,"VALVE, BALL: VALVE SIZE: 25 MM; DESIGN RATING: 63; TEMPERATURE RATING: 200 DEG C; CONNECTION: FEMALE THD; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 90 MM; OPERATED: HAND; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: PTFE; SPECIFICATION: JT97AN; PORT TYPE: BALL; APPLICATION: VARIOUS; GRADE: 1.4408; TYPE: ISOLATING","PARKER, PISTER, KLINGER MZANSI","BALL; ISOLATING","25 MM","STAINLESS STEEL",63,"STAINLESS STEEL","FEMALE THD","90 MM","N/A","HAND","VARIOUS","200 DEG C",null,null,"PTFE"]
["Ingula Pumped Storage Scheme",619983,"VALVE, BALL: VALVE SIZE: 50 MM; DESIGN RATING: 10 KPA; TEMPERATURE RATING: JIS10K; CONNECTION: FLANGED; BODY MATERIAL: SCPH2/304; FACE TO FACE LENGTH: 175 MM; OPERATED: LEVER; STYLE: DIRECTIONAL; TRIM: STL; SOFTGOODS: PTFE; APPLICATION: UPPER OIL COOLER; TYPE: ISOLATING","PARKER, PISTER, KLINGER MZANSI","BALL; ISOLATING","50 MM","SCPH2/304","10 KPA","STL","FLANGED","175 MM","120 MM","LEVER","UPPER OIL COOLER","JIS10K",null,null,"PTFE"]
["Ingula Pumped Storage Scheme",628694,"VALVE, BALL: VALVE SIZE: 50 MM; DESIGN RATING: 63 BAR; TEMPERATURE RATING: 200 DEG C; CONNECTION: FEMALE THD; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 140 MM; OPERATED: HAND; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: PTFE; SPECIFICATION: JT97AN; PORT TYPE: BALL; APPLICATION: VARIOUS; GRADE: 1.4408; TYPE: ISOLATING","PARKER, PISTER, KLINGER MZANSI","BALL; ISOLATING","50 MM","STAINLESS STEEL","63 BAR","STAINLESS STEEL","FEMALE THD","140 MM","N/A","HAND","VARIOUS","200 DEG C",null,null,"PTFE"]
["Ingula Pumped Storage Scheme",637421,"VALVE, BALL: VALVE SIZE: DN 100; DESIGN RATING: PN100; TEMPERATURE RATING: -10 TO 50 DEG C; CONNECTION: FLANGE; BODY MATERIAL: 1.4571; OPERATED: LEVER; SPECIFICATION: SAE; DIN; ANSI; ISO; TYPE: PNEUMATIC; REFERENCE NO: 190-100-202; .","PARKER, PISTER, KLINGER MZANSI, VOITH","BALL; PNEUMATIC","DN 100",1.4571,"PN100","STAINLESS STEEL","FLANGE","≈ 230 mm","190 MM","LEVER","HYDRAULIC AND PNEUMATIC SYSTEMS, WATER SERVICES, GASES, LIGHT CHEMICAL FLUIDS","-10 TO 50 DEG C","190-100-202"]
["Ingula Pumped Storage Scheme",648284,"VALVE: TYPE: EMERGENCY CLOSING; VALVE SIZE: 13 MM; DESIGN RATING: 350 BAR; TEMPERATURE RATING: 200 DEG C; FACE TO FACE LENGTH: FLAT; CONNECTION: THREADED; OPERATED: PRESSURE; BODY MATERIAL: STEEL; STYLE: 2 WAY; SPECIFICATION: ISO 9001; TURBINE GOVERNOR PUMP CONTROL; KKS: MFX20AA201/219","VOITH","EMERGENCY CLOSING","13 MM","STEEL","350 BAR","STAINLESS STEEL","THREADED","FLAT","N/A","PRESSURE","HIGH PRESSURE HYDRAULIC OIL, TURBINE GOVERNOR OIL SYSTEM","200 DEG C"]
["Ingula Pumped Storage Scheme",646934,"VALVE: TYPE: DIRECTIONAL; VALVE SIZE: NG 6; DESIGN RATING: 350 BAR; TEMPERATURE RATING: -25 TO 70 DEG C; FACE TO FACE LENGTH: FLANGE; CONNECTION: SUBPLATE; OPERATED: HAND; BODY MATERIAL: CARBON STEEL; STYLE: 4/2 WAY; TRIM: STAINLESS STEEL; SPECIFICATION: ISO 4401-03; SOFTGOODS: NBR; MANUF P/N: AH4Z60A/R-Z80",null,"DIRECTIONAL","NG 6","CARBON STEEL","350 BAR","STAINLESS STEEL","SUBPLATE","FLANGE",null,"HAND",null,"-25 TO 70 DEG C","AH4Z60A/R-Z80",null,"NBR"]
["Ingula Pumped Storage Scheme",642473,"VALVE: TYPE: DIRECTIONAL; VALVE SIZE: 8/4 MM; DESIGN RATING: 350 BAR; TEMPERATURE RATING: 52 DEG C; FACE TO FACE LENGTH: 49 MM; CONNECTION: BOLT BLOCK; OPERATED: PRESSURE; BODY MATERIAL: STEEL; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SPECIFICATION: ISO 4401-03; SOFTGOODS: NBR; SPECIAL FEATURES: NIL; MANUF P/N: WDMFA06-AB3-G220/MD-HF1-P1AB",null,"DIRECTIONAL","8/4 MM","STEEL","350 BAR","STAINLESS STEEL","BOLT BLOCK","49 MM",null,"PRESSURE",null,"52 DEG C","WDMFA06-AB3-G220/MD-HF1-P1AB",null,"NBR"]
["Ingula Pumped Storage Scheme",637416,"VALVE: TYPE: SAFETY; VALVE SIZE: DN40; DESIGN RATING: 35 BAR; TEMPERATURE RATING: 20 DEG C; CONNECTION: FLANGE INLET P 40, OUTLET PN16; OPERATED: HAND LEVER; BODY MATERIAL: 1.4408; SPECIFICATION: 4414.4664; REFERENCE NO: 10944010; CENTER TO FACE: INLET 140 MM, OUTLET 115 MM","LESER,REXROTH,ENERGY VALVES,","SAFETY","DN40",1.4408,"35 BAR","STAINLESS STEEL","FLANGE INLET P 40, OUTLET PN16","n/a","110 MM","HAND LEVER",null,"20 DEG C",10944010]
["Ingula Pumped Storage Scheme",630729,"VALVE: TYPE: ISOLATING GAUGE; VALVE SIZE: DN 4; DESIGN RATING: PN400; TEMPERATURE RATING: -20 TO 200 DEG C; FACE TO FACE LENGTH: 140 MM; CONNECTION: THD MALE X FEMALE; OPERATED: HANDWHEEL; BODY MATERIAL: STAINLESS STEEL; STYLE: 2 WAY; GRADE: 1.4571; SPECIAL FEATURES: VENT SCREW","PAKER, SUPERPUMP , HYDRAULICS, PISTER","ISOLATING GAUGE","DN 4","STAINLESS STEEL","PN400","STAINLESS STEEL","THD MALE X FEMALE","140 MM","N/A","HANDWHEEL",null,"-20 TO 200 DEG C"]
["Ingula Pumped Storage Scheme",630728,"VALVE: TYPE: ISOLATING GAUGE; VALVE SIZE: DN 4; TEMPERATURE RATING: -20 TO 200 DEG C; FACE TO FACE LENGTH: 140 MM; CONNECTION: THD MALE X FEMALE; OPERATED: HANDWHEEL; BODY MATERIAL: STAINLESS STEEL; STYLE: 3 WAY; GRADE: 1.4571; SPECIAL FEATURES: VENT SCREW","PAKER, SUPERPUMP , HYDRAULICS, PISTER","ISOLATING GAUGE","DN 4","STAINLESS STEEL","PN400","STAINLESS STEEL","THD MALE X FEMALE","140 MM","N/A","HANDWHEEL","HYDRAULIC OIL","-20 TO 200 DEG C"]
["Ingula Pumped Storage Scheme",72645,"VALVE: TYPE: HYDRAULIC; VALVE SIZE: 3/4 IN","PISTER/UFIXED/HYDEC","HYDRAULIC","3/4 IN","STAINLESS STEEL","PN315","STAINLESS STEEL, ","THREADED","≈ 70 – 120 mm","N/A","MANUALLY","HYDRAULIC OIL","–20°C to +80°C"]
["Ingula Pumped Storage Scheme",644906,"VALVE, CHECK: TYPE: DUAL PURPOSE; VALVE SIZE: 1-1/2 IN; DESIGN RATING: 3000 PSI; TEMPERATURE RATING: -30 TO 80 DEG C; CONNECTION: INSERT; BODY MATERIAL: STEEL; FACE TO FACE LENGTH: 65 MM; OPERATED: PRESSURE; STYLE: 1 WAY; TRIM: BRASS; SOFTGOODS: NITRILE; APPLICATION: SAE FLANGE PORT; SPECIFICATION: ISO 9001; GRADE: HT; MANUF P/N: RVSAE3-112-5 13K","VALVES FOR AFRIKA,SUPERPUMP, KLINGER MZANSI","CHECK; DUAL PURPOSE","1-1/2 IN","STEEL","3000 PSI","BRASS","INSERT","65 MM","N/A","PRESSURE","SAE FLANGE PORT","-30 TO 80 DEG C","RVSAE3-112-5 13K",null,"NITRILE"]
["Ingula Pumped Storage Scheme",628680,"VALVE, CHECK: TYPE: DISC; VALVE SIZE: DN 80; DESIGN RATING: PN40; TEMPERATURE RATING: -200 TO 550 DEG C; CONNECTION: FLANGE; BODY MATERIAL: CI 300; FACE TO FACE LENGTH: 50 MM; OPERATED: FLOW; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: STAINLESS STEEL; APPLICATION: VARIOUS; SPECIFICATION: (PED) 97/23/EC; GRADE: 1.4408; MANUF P/N: RK86A; WITH BODY CENTERING CAMS; FLOWSERVE","VALVES FOR AFRIKA,SUPERPUMP, KLINGER MZANSI","CHECK; DISC","DN 80","CI 300","PN40","STAINLESS STEEL","FLANGE","50 MM","160 mm","FLOW","VARIOUS","-200 TO 550 DEG C","RK86A",null,"STAINLESS STEEL"]
["Ingula Pumped Storage Scheme",644902,"VALVE: TYPE: DIRECTIONAL PISTON; VALVE SIZE: NG10; DESIGN RATING: 315 BAR; TEMPERATURE RATING: -5 TO 50 DEG C; FACE TO FACE LENGTH: NIL; CONNECTION: MOUNTING PLATE; OPERATED: ELECTRIC; BODY MATERIAL: CAST IRON; STYLE: 4/2 WAY; TRIM: STAINLESS STEEL; GRADE: NIL; SPECIFICATION: ISO 9001; SOFTGOODS: NBR; SPECIAL FEATURES: NIL; MANUF P/N: WE02-10P100E220/CHN",null,"DIRECTIONAL PISTON","NG10","CAST IRON","315 BAR","STAINLESS STEEL","MOUNTING PLATE","NIL",null,"ELECTRIC",null,"-5 TO 50 DEG C","WE02-10P100E220/CHN",null,"NBR"]
["Ingula Pumped Storage Scheme",623858,"VALVE, CHECK: TYPE: FLOW CONTROL; VALVE SIZE: NS16; DESIGN RATING: 1.5 BAR; TEMPERATURE RATING: -20 TO 80 DEG C; CONNECTION: FLANGE; BODY MATERIAL: CI; FACE TO FACE LENGTH: 70 MM; OPERATED: PILOT; STYLE: 2 WAY; APPLICATION: SURGE CHAMBER HOIST; SPECIFICATION: DIN 51524; OEM P/N: 2FRM16-32/160L, OEM: BOSCH REXROTH; LOCKABLE; FLOW RATE: 160 L/MIN.","Bosch; Rexroth","CHECK; FLOW CONTROL","NS16","CI","1.5 BAR","HARDENED STEEL","FLANGE","70 MM","N/A","PILOT","SURGE CHAMBER HOIST","-20 TO 80 DEG C","2FRM16-32/160L, OEM: BOSCH REXROTH"]
["Ingula Pumped Storage Scheme",623859,"VALVE, CHECK: TYPE: FLOW CONTROL; VALVE SIZE: NS10; DESIGN RATING: 1.5 BAR; TEMPERATURE RATING: -20 TO 80 DEG C; CONNECTION: FLANGE; BODY MATERIAL: CI; FACE TO FACE LENGTH: 55 MM; OPERATED: PILOT; STYLE: 2 WAY; APPLICATION: SURGE CHAMBER HOIST; SPECIFICATION: DIN 51524; OEM P/N: 2FRM10-31/50L, OEM: BOSCH REXROTH; LOCKABLE; FLOW RATE: 50 L/MIN.","Bosch; Rexroth","CHECK; FLOW CONTROL","NS10","CI","1.5 BAR","HARDENED STEEL","FLANGE","55 MM","N/A","PILOT","SURGE CHAMBER HOIST","-20 TO 80 DEG C","2FRM10-31/50L, OEM: BOSCH REXROTH"]
["Ingula Pumped Storage Scheme",178003,"VALVE, CHECK: VALVE SIZE: 100 MM; DESIGN RATING: 3-8 BAR; TEMPERATURE RATING: 50-100 DEG C; MANUF P/N: NINSSC 0100; .","SUPERPUMP, KLINGER MZANSI","CHECK","100 MM","CAST IRON AND DUCTILE","3-8 BAR","STAINLESS STEEL","FLANGE","≈ 350 MM","180 MM","VARIOUS","WATER, HOT WATER AND CLEAN INDUSTRIAL FLUIDS","50-100 DEG C","NINSSC 0100"]
["Ingula Pumped Storage Scheme",628204,"VALVE, BUTTERFLY: TYPE: WAFER; VALVE SIZE: DN65; DESIGN RATING: 16 BAR; TEMPERATURE RATING: -40 TO 200 DEG C; CONNECTION: CENTER FLANGE; BODY MATERIAL: CI; FACE TO FACE LENGTH: 46 MM; OPERATED: LEVERLOCK; TRIM: STAINLESS STEEL; SOFTGOODS: NBR; APPLICATION: WATER; GRADE: 1.4409; SPECIFICATION: EN ISO 5211; STYLE: CENTERED DISC; SCHEDULE: EN 558 SERIES 20; SPECIAL FEATURES: NONE; MANUF P/N: Z011-A","SUPERPUMP, KLINGER MZANSI","BUTTERFLY; WAFER","DN65","CI","16 BAR","STAINLESS STEEL","CENTER FLANGE","46 MM","145 MM","LEVERLOCK","WATER","-40 TO 200 DEG C","Z011-A",null,"NBR"]
["Ingula Pumped Storage Scheme",643980,"VALVE, BUTTERFLY: TYPE: WAFER; VALVE SIZE: DN40; DESIGN RATING: 16 BAR; TEMPERATURE RATING: 200 DEG C; CONNECTION: FLANGE; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 33 MM; OPERATED: LEVER; TRIM: STAINLESS STEEL; SOFTGOODS: EPDM; APPLICATION: BLOWDOWN; GRADE: 1.4408; SPECIFICATION: EN 1092-1; STYLE: 1 WAY; SPECIAL FEATURES: ADJUSTABLE POSITION; MANUF P/N: Z011-A; CF8M; EBRO","SUPERPUMP, KLINGER MZANSI","BUTTERFLY; WAFER","DN40","STAINLESS STEEL","16 BAR","STAINLESS STEEL","FLANGE","33 MM","110 MM","LEVER","BLOWDOWN","200 DEG C","Z011-A",null,"EPDM"]
["Ingula Pumped Storage Scheme",623861,"VALVE, CHECK: TYPE: FLOW CONTROL; VALVE SIZE: 1 IN; DESIGN RATING: 320 BAR; TEMPERATURE RATING: -20 TO 100 DEG C; CONNECTION: THD; BODY MATERIAL: STEEL; FACE TO FACE LENGTH: 117 MM; OPERATED: PRESSURE, 0 BAR; STYLE: 1 WAY; APPLICATION: SURGE CHAMBER HOIST; SPECIFICATION: EN 10083; OEM P/N: FT257/6 100 0 BAR; SPRING REMOVED","SUPERPUMP, KLINGER MZANSI","CHECK; FLOW CONTROL","1 IN","STEEL","320 BAR","STEEL AND HARDENED STEEL","THD","117 MM","N/A","PRESSURE, 0 BAR","SURGE CHAMBER HOIST","-20 TO 100 DEG C","FT257/6 100 0 BAR"]
["Ingula Pumped Storage Scheme",692898,"VALVE, SOLENOID: PIPE SIZE: 1/2 IN; STYLE: 1/1; POTENTIAL: 220 VDC; DESIGN RATING: 0-1.5 MPA; CONNECTION: BSPF; BODY MATERIAL: BRASS; OPERATED: SOLENOID; ENCLOSURE RATING: IP65; MEDIUM: AIR; ORIFICE SIZE: 3 MM; COIL: SINGLE; APPLICATION: MECHANICAL AIR BRAKE SYSTEM; OEM P/N: VS3P-4030-10G HMJ-X","VALVES FOR AFRIKA,SUPERPUMP, KLINGER MZANSI","SOLENOID","1/2 IN; 3 MM","BRASS","0-1.5 MPA","STAINLESS AND BRASS","BSPF","60 - 80 MM","PCD","SOLENOID","AIR; MECHANICAL AIR BRAKE SYSTEM","–10°C to +80°C","VS3P-4030-10G HMJ-X","220 VDC; SINGLE; IP65"]
["Ingula Pumped Storage Scheme",692543,"VALVE: TYPE: NON RETURN; VALVE SIZE: 20 MM; TEMPERATURE RATING: -10 TO 100 DEG C; CONNECTION: 1/2 IN-BSP; OPERATED: AIR; BODY MATERIAL: STAINLESS STEEL; OEM P/N: 033930","SAUER COMPRESSOR","NON RETURN","20 MM","STAINLESS STEEL","PN16","STAINLESS STEEL ","1/2 IN-BSP","50 - 70 MM","N/A","AIR","COMPRESSED AIR","-10 TO 100 DEG C",33930]
["Ingula Pumped Storage Scheme",628662,"VALVE: TYPE: SAFETY; VALVE SIZE: 4 IN; DESIGN RATING: 53 BAR; TEMPERATURE RATING: 538 DEG C; CONNECTION: FLANGE; OPERATED: PRESSURE, SPRING, 0-35 LB; BODY MATERIAL: BS 1504-240; STYLE: ANGLE PATTERN; TRIM: PT; OEM P/N: 4\"707 SD; DRAWING NO: F5217/5 REV 0; .","LESER,REXROTH","SAFETY","4 IN","BS 1504-240","53 BAR","PT","FLANGE","320 - 400 MM","190 MM","PRESSURE, SPRING, 0-35 LB","STEAM","538 DEG C","4\"707 SD; F5217/5 REV 0"]
["Ingula Pumped Storage Scheme",619975,"VALVE: TYPE: SHUT OFF; VALVE SIZE: 3/8 IN; DESIGN RATING: 200 BAR; TEMPERATURE RATING: -10 TO 120 DEG C; FACE TO FACE LENGTH: 55 MM; CONNECTION: BSP SCREW; OPERATED: HAND; BODY MATERIAL: BRASS; STYLE: 3 WAY; OEM P/N: CA200MP; TYPE ASK","ASK","SHUT OFF","3/8 IN","BRASS","200 BAR","STAINLESS STEEL","BSP SCREW","55 MM","N/A","HAND","HYDRAULIC OIL, COMPRESSED AIR","-10 TO 120 DEG C","CA200MP"]
["Ingula Pumped Storage Scheme",41833,"VALVE: TYPE: COMPRESSOR; VALVE SIZE: 175 MM; OPERATED: PRESSURE; BODY MATERIAL: STL; TRIM: DISC SS; 2ND STAGE CONCENTRIC","SAUER COMPRESSOR","COMPRESSOR","175 MM","STL","27BAR","DISC SS","N/A","N/A","N/A","PRESSURE","COMPRESSED AIR","50 DEG C"]
["Ingula Pumped Storage Scheme",637382,"VALVE: TYPE: CONCENTRIC; VALVE SIZE: OD 225 X THK 30 MM; DESIGN RATING: 380 BAR; TEMPERATURE RATING: -28 TO 425 DEG C; CONNECTION: SEAT; OPERATED: MECHANICAL; BODY MATERIAL: STAINLESS STEEL; STYLE: LEAF; MANUF P/N: 37134; MODEL NO: WP6310; FOR USE ON JP SAUER AND SOHN COMPRESSOR","SAUER COMPRESSOR","CONCENTRIC","OD 225 X THK 30 MM","STAINLESS STEEL","380 BAR","STAINLESS STEEL","SEAT","N/A","N/A","MECHANICAL","JP SAUER AND SOHN COMPRESSOR","-28 TO 425 DEG C","37134; WP6310"]
["Ingula Pumped Storage Scheme",701459,"VALVE: TYPE: CONTROL; VALVE SIZE: NG10; DESIGN RATING: 120 BAR; TEMPERATURE RATING: 20-60 DEG C; CONNECTION: FLANGE; OPERATED: CONTINUOUSLY; BODY MATERIAL: STEEL; STYLE: BLOCK CM2; PROFIBUS DP STANDARD I6C61158 R24KX2F3H592-BDK2D1 MODEL: D637-1033-0001",null,"CONTROL","NG10","STEEL","120 BAR",null,"FLANGE",null,null,"CONTINUOUSLY",null,"20-60 DEG C"]
["Ingula Pumped Storage Scheme",644954,"VALVE: TYPE: DIRECTIONAL CONTROL; VALVE SIZE: 6 MM; DESIGN RATING: 350 BAR; TEMPERATURE RATING: -30 TO 80 DEG C; FACE TO FACE LENGTH: NIL; CONNECTION: SUBPLATE; OPERATED: SOLENOID; BODY MATERIAL: STEEL; STYLE: 4/2 WAY; TRIM: METAL; SPECIFICATION: ISO 9001; SOFTGOODS: NBR; SPECIAL FEATURES: WITH RNEH5-162R11/22000E1 SUBPLATE; MANUF P/N: RPE3-06R11/22000E1",null,"DIRECTIONAL CONTROL","6 MM","STEEL","350 BAR","METAL","SUBPLATE","NIL",null,"SOLENOID",null,"-30 TO 80 DEG C","RPE3-06R11/22000E1",null,"NBR"]
["Ingula Pumped Storage Scheme",623860,"VALVE, CHECK: TYPE: FLOW CONTROL; VALVE SIZE: 1-1/4 IN; DESIGN RATING: 320 BAR; TEMPERATURE RATING: -20 TO 100 DEG C; CONNECTION: THD; BODY MATERIAL: STEEL; FACE TO FACE LENGTH: 134.5 MM; OPERATED: PRESSURE, 1 BAR; STYLE: 1 WAY; APPLICATION: SURGE CHAMBER HOIST; SPECIFICATION: EN 10083; OEM P/N: FT257/6 114 1 BAR","SUPERSUMP, KLINGERMZANSI, VALVES FOR AFRICA","CHECK; FLOW CONTROL","1-1/4 IN","STEEL","320 BAR","HARDENED STEEL","THD","134.5 MM","N/A","PRESSURE, 1 BAR","SURGE CHAMBER HOIST","-20 TO 100 DEG C","FT257/6 114 1 BAR"]
["Ingula Pumped Storage Scheme",731181,"VALVE, CHECK: TYPE: E65; VALVE SIZE: DN25 MM; DESIGN RATING: PN40; TEMPERATURE RATING: -20to70 degree; CONNECTION: FLANGE; BODY MATERIAL: CAST IRON; FACE TO FACE LENGTH: 0.01 M; OPERATED: ELECTRICAL ACTUATOR","VALVES FOR AFRIKA,SUPERPUMP, KLINGER MZANSI","CHECK; E65","DN25 MM","CAST IRON","PN40","STAINLESS STEEL","FLANGE","0.01 M","85 MM","ELECTRICAL ACTUATOR","WATER","-20to70 degree"]
["Ingula Pumped Storage Scheme",644907,"VALVE, CHECK: TYPE: DUAL PURPOSE; VALVE SIZE: 2-1/2 IN; DESIGN RATING: 3000 PSI; TEMPERATURE RATING: -30 TO 80 DEG C; CONNECTION: INSERT; BODY MATERIAL: STEEL; FACE TO FACE LENGTH: 85 MM; OPERATED: PRESSURE; STYLE: 1 WAY; TRIM: BRASS; SOFTGOODS: NITRILE; APPLICATION: SAE FLANGE PORT; SPECIFICATION: ISO 9001; GRADE: HT; MANUF P/N: RVSAE3DS-212-4","PISTER, PAKER ,KLINGER MZANSI, SUPERPUMP","CHECK; DUAL PURPOSE","2-1/2 IN","STEEL","3000 PSI","BRASS","INSERT","85 MM","127 MM","PRESSURE","SAE FLANGE PORT","-30 TO 80 DEG C","RVSAE3DS-212-4",null,"NITRILE"]
["Ingula Pumped Storage Scheme",655868,"VALVE, BUTTERFLY: TYPE: WAFER; VALVE SIZE: 250 MM; DESIGN RATING: PN100; TEMPERATURE RATING: -20 TO 200 DEG F; CONNECTION: FLANGE; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 235 MM; OPERATED: HANDWHEEL/GEARBOX; TRIM: STAINLESS STEEL; SOFTGOODS: PTFE; APPLICATION: VARIOUS; GRADE: 1.4408; STYLE: 1 WAY; REFERENCE NO: 1-MF-A10-060 G00; COMPLETE WITH ROTORK GEARBOX AB880N; LEUSCH LTR43","PISTER, PAKER ,KLINGER MZANSI, SUPERPUMP, VALVES FOR AFRICA","BUTTERFLY; WAFER","250 MM","STAINLESS STEEL","PN100","STAINLESS STEEL","FLANGE","235 MM","405 MM","HANDWHEEL/GEARBOX","VARIOUS","-20 TO 200 DEG F","1-MF-A10-060 G00",null,"PTFE"]
["Ingula Pumped Storage Scheme",628207,"VALVE, BUTTERFLY: TYPE: WAFER; VALVE SIZE: DN125; DESIGN RATING: 16 BAR; TEMPERATURE RATING: -40 TO 200 DEG C; CONNECTION: CENTER FLANGE; BODY MATERIAL: CI; FACE TO FACE LENGTH: 56 MM; OPERATED: LEVERLOCK; TRIM: STAINLESS STEEL; SOFTGOODS: NBR; APPLICATION: WATER; GRADE: 1.4409; SPECIFICATION: EN ISO 5211; STYLE: CENTERED DISC; SCHEDULE: EN 558 SERIES 20; SPECIAL FEATURES: NONE; MANUF P/N: Z011-A","PISTER, PAKER ,KLINGER MZANSI, SUPERPUMP,VALVES FOR AFRICA","BUTTERFLY; WAFER","DN125","CI","16 BAR","STAINLESS STEEL","CENTER FLANGE","56 MM","210 MM","LEVERLOCK","WATER","-40 TO 200 DEG C","Z011-A",null,"NBR"]
["Ingula Pumped Storage Scheme",628203,"VALVE, BUTTERFLY: TYPE: WAFER; VALVE SIZE: DN 50; DESIGN RATING: 10 BAR; TEMPERATURE RATING: -40 TO 200 DEG C; CONNECTION: CENTER FLANGE; BODY MATERIAL: CI; FACE TO FACE LENGTH: 43 MM; OPERATED: LEVERLOCK; TRIM: STAINLESS STEEL; SOFTGOODS: NBR; APPLICATION: WATER; GRADE: 1.4409; SPECIFICATION: EN ISO 5211; STYLE: CENTERED DISC; SCHEDULE: EN 558 SERIES 20; SPECIAL FEATURES: NONE; MANUF P/N: Z011-A; .","PISTER, PAKER ,KLINGER MZANSI, SUPERPUMP,VALVES FOR AFTICA","BUTTERFLY; WAFER","DN 50","CI","10 BAR","STAINLESS STEEL","CENTER FLANGE","43 MM","125 MM","LEVERLOCK","WATER","-40 TO 200 DEG C","Z011-A",null,"NBR"]
["Ingula Pumped Storage Scheme",628205,"VALVE, BUTTERFLY: TYPE: WAFER; VALVE SIZE: 80 MM; DESIGN RATING: 10 BAR; TEMPERATURE RATING: -40 TO 200 DEG C; CONNECTION: CENTER FLANGE; BODY MATERIAL: CI; FACE TO FACE LENGTH: 46 MM; OPERATED: LEVERLOCK; TRIM: STAINLESS STEEL; SOFTGOODS: NBR; APPLICATION: WATER; GRADE: 1.4409; SPECIFICATION: EN ISO 5211; STYLE: CENTERED DISC; SCHEDULE: EN 558 SERIES 20; SPECIAL FEATURES: NONE; MANUF P/N: Z011-A","PISTER, PAKER ,KLINGER MZANSI, SUPERPUMP,VALVES FOR AFTICA","BUTTERFLY; WAFER","80 MM","CI","10 BAR","STAINLESS STEEL","CENTER FLANGE","46 MM","`160 MM","LEVERLOCK","WATER","-40 TO 200 DEG C","Z011-A",null,"NBR"]
["Ingula Pumped Storage Scheme",657949,"VALVE, BALL: VALVE SIZE: DN125; DESIGN RATING: PN16; TEMPERATURE RATING: 40 DEG C; CONNECTION: FLANGE; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 235 MM; OPERATED: ACTUATOR; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: PTFE; SPECIFICATION: ISO 9001; PORT TYPE: SCREW; APPLICATION: TURBINE; GRADE: 1.4301; TYPE: SHUT OFF; MODEL NO: FCKH; REFERENCE NO: 4423; WITH ROTORK ACTUATOR MODEL AB880M; PISTER.","WITH ROTORK ACTUATOR","BALL; SCREW; SHUT OFF","DN125","STAINLESS STEEL","PN16","STAINLESS STEEL","FLANGE","235 MM","210 MM","ACTUATOR","TURBINE","40 DEG C","4423; FCKH",null,"PTFE"]
["Ingula Pumped Storage Scheme",657948,"VALVE, BALL: VALVE SIZE: DN125; DESIGN RATING: PN100; TEMPERATURE RATING: 2-40 DEG C; CONNECTION: FLANGE; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 400 MM; OPERATED: ACTUATOR; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: PTFE; SPECIFICATION: ISO 9001; PORT TYPE: SCREW; APPLICATION: TURBINE; GRADE: 1.4301; TYPE: SHUT OFF; MODEL NO: FCKH; REFERENCE NO: 9423 486/13; COMPLETE WITH EXTENSION PART NUMBER 98651 P1 AND ROTORK ACTUATOR MODEL AB880M; PISTER.","PISTER, PAKER ,KLINGER MZANSI, SUPERPUMP,VALVES FOR AFTICA","BALL; SCREW; SHUT OFF","DN125","STAINLESS STEEL","PN100","STAINLESS STEEL","FLANGE","400 MM","250 MM","ACTUATOR","TURBINE","2-40 DEG C","9423 486/13; FCKH",null,"PTFE"]
["Ingula Pumped Storage Scheme",657950,"VALVE, BALL: VALVE SIZE: DN65; DESIGN RATING: PN100; TEMPERATURE RATING: 0-40 DEG C; CONNECTION: FLANGE; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 130 MM; OPERATED: ACTUATOR/LEVER; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: PTFE; SPECIFICATION: ISO 9001; PORT TYPE: SCREW; APPLICATION: TURBINE; GRADE: 1.4301; TYPE: SHUT OFF; MODEL NO: FCKH; REFERENCE NO: 9423 453/13; PISTER.","PISTER, PAKER ,KLINGER MZANSI, SUPERPUMP,VALVES FOR AFTICA","BALL; SCREW; SHUT OFF","DN65","STAINLESS STEEL","PN100","STAINLESS STEEL","FLANGE","130 MM","185 MM","ACTUATOR/LEVER","TURBINE","0-40 DEG C","9423 453/13; FCKH",null,"PTFE"]
["Ingula Pumped Storage Scheme",655832,"VALVE, BUTTERFLY: TYPE: WAFER; VALVE SIZE: 200 MM; DESIGN RATING: PN 16; TEMPERATURE RATING: -20 TO 200 DEG C; CONNECTION: FLANGE; BODY MATERIAL: CI; FACE TO FACE LENGTH: 60 MM; OPERATED: HANDWHEEL; TRIM: STAINLESS STEEL; SOFTGOODS: NBR; APPLICATION: VARIOUS; GRADE: 316; SPECIFICATION: ISO 9001; STYLE: 1 WAY; EBRO ARMATUREN","PISTER, PAKER ,KLINGER MZANSI, SUPERPUMP,VALVES FOR AFTICA","BUTTERFLY; WAFER","200 MM","CI","PN 16","STAINLESS STEEL","FLANGE","60 MM","295 MM","HANDWHEEL","VARIOUS","-20 TO 200 DEG C",null,null,"NBR"]
["Ingula Pumped Storage Scheme",655865,"VALVE, BUTTERFLY: TYPE: WAFER; VALVE SIZE: 150 MM; DESIGN RATING: PN40; TEMPERATURE RATING: -20 TO 200 DEG F; CONNECTION: FLANGE; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 55 MM; OPERATED: HANDWHEEL; TRIM: STAINLESS STEEL; SOFTGOODS: PTFE; APPLICATION: VARIOUS; GRADE: 1.4408; STYLE: 1 WAY; EBRO ARMATUREN","PISTER, PAKER ,KLINGER MZANSI, SUPERPUMP,VALVES FOR AFTICA","BUTTERFLY; WAFER","150 MM","STAINLESS STEEL","PN40","STAINLESS STEEL","FLANGE","55 MM","285 MM","HANDWHEEL","VARIOUS","-20 TO 200 DEG F",null,null,"PTFE"]
["Ingula Pumped Storage Scheme",620187,"VALVE, BALL: VALVE SIZE: 1/2 IN; DESIGN RATING: 1 MPA; TEMPERATURE RATING: 100 DEG C; CONNECTION: MALE X FEMALE 1/2 IN; BODY MATERIAL: STEEL; FACE TO FACE LENGTH: 90 MM; OPERATED: LEVER; TYPE: SHUT OFF; OEM P/N: X13W-40P; YONP","PISTER, PARKER,HYDEC","BALL; SHUT OFF","1/2 IN","STEEL","1 MPA","STAINLESS STEEL, CARBON STEEL","MALE X FEMALE 1/2 IN","90 MM","N/A","LEVER","COOLING WATER, SERVICE WATER, HYDRAULIC OIL","100 DEG C","X13W-40P"]
["Ingula Pumped Storage Scheme",655834,"VALVE, BUTTERFLY: TYPE: WAFER; VALVE SIZE: 600 MM; DESIGN RATING: PN 16; TEMPERATURE RATING: -20 TO 200 DEG C; CONNECTION: FLANGE; BODY MATERIAL: CI; FACE TO FACE LENGTH: 140 MM; OPERATED: HANDWHEEL; TRIM: STAINLESS STEEL; SOFTGOODS: EPDM 80 KTW; APPLICATION: VARIOUS; GRADE: 316; SPECIFICATION: ISO 9001; STYLE: 1 WAY; COMPLETE WITH ROTORK GEARBOX MODEL AB8600N/SP4; EBRO ARMATUREN","COMPLETE WITH ROTORK GEARBOX","BUTTERFLY; WAFER","600 MM","CI","PN 16","STAINLESS STEEL","FLANGE","140 MM","840 MM","HANDWHEEL","VARIOUS","-20 TO 200 DEG C",null,null,"EPDM 80 KTW"]
["Ingula Pumped Storage Scheme",655831,"VALVE, BUTTERFLY: TYPE: WAFER; VALVE SIZE: 300 MM; DESIGN RATING: PN 16; TEMPERATURE RATING: -20 TO 200 DEG C; CONNECTION: FLANGE; BODY MATERIAL: CI; FACE TO FACE LENGTH: 90 MM; OPERATED: HANDWHEEL; TRIM: STAINLESS STEEL; SOFTGOODS: NBR; APPLICATION: VARIOUS; GRADE: 316; SPECIFICATION: ISO 9001; STYLE: 1 WAY; EBRO ARMATUREN","PISTER, PAKER ,KLINGER MZANSI, SUPERPUMP,VALVES FOR AFTICA","BUTTERFLY; WAFER","300 MM","CI","PN 16","STAINLESS STEEL","FLANGE","90 MM","410 MM","HANDWHEEL","VARIOUS","-20 TO 200 DEG C",null,null,"NBR"]
["Ingula Pumped Storage Scheme",655867,"VALVE, BUTTERFLY: TYPE: WAFER; VALVE SIZE: 300 MM; DESIGN RATING: PN25; TEMPERATURE RATING: -20 TO 200 DEG F; CONNECTION: FLANGE; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 77 MM; OPERATED: HANDWHEEL; TRIM: STAINLESS STEEL; SOFTGOODS: PTFE; APPLICATION: VARIOUS; GRADE: 1.4408; STYLE: 1 WAY; EBRO ARMATUREN","PISTER, PAKER ,KLINGER MZANSI, SUPERPUMP,VALVES FOR AFTICA","BUTTERFLY; WAFER","300 MM","STAINLESS STEEL","PN25","STAINLESS STEEL","FLANGE","77 MM","460 MM","HANDWHEEL","VARIOUS","-20 TO 200 DEG F",null,null,"PTFE"]
["Ingula Pumped Storage Scheme",655833,"VALVE, BUTTERFLY: TYPE: WAFER; VALVE SIZE: 150 MM; DESIGN RATING: PN 16; TEMPERATURE RATING: -20 TO 200 DEG C; CONNECTION: FLANGE; BODY MATERIAL: CI; FACE TO FACE LENGTH: 55 MM; OPERATED: LEVER; TRIM: STAINLESS STEEL; SOFTGOODS: NBR; APPLICATION: VARIOUS; GRADE: 316; SPECIFICATION: ISO 9001; STYLE: 1 WAY; EBRO ARMATUREN","PISTER, PAKER ,KLINGER MZANSI, SUPERPUMP,VALVES FOR AFTICA","BUTTERFLY; WAFER","150 MM","CI","PN 16","STAINLESS STEEL","FLANGE","55 MM","240 MM","LEVER","VARIOUS","-20 TO 200 DEG C",null,null,"NBR"]
["Ingula Pumped Storage Scheme",655866,"VALVE, BUTTERFLY: TYPE: WAFER; VALVE SIZE: 200 MM; DESIGN RATING: PN40; TEMPERATURE RATING: -20 TO 200 DEG F; CONNECTION: FLANGE; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 60 MM; OPERATED: HANDWHEEL; TRIM: STAINLESS STEEL; SOFTGOODS: PTFE; APPLICATION: VARIOUS; GRADE: 1.4408; STYLE: 1 WAY; EBRO ARMATUREN","PISTER, PAKER ,KLINGER MZANSI, SUPERPUMP,VALVES FOR AFTICA","BUTTERFLY; WAFER","200 MM","STAINLESS STEEL","PN40","STAINLESS STEEL","FLANGE","60 MM","375 MM","HANDWHEEL","VARIOUS","-20 TO 200 DEG F",null,null,"PTFE"]
["Ingula Pumped Storage Scheme",628206,"VALVE, BUTTERFLY: TYPE: WAFER; VALVE SIZE: DN 100; DESIGN RATING: 10 BAR; TEMPERATURE RATING: -40 TO 200 DEG C; CONNECTION: CENTER FLANGE; BODY MATERIAL: CI; FACE TO FACE LENGTH: 52 MM; OPERATED: LEVERLOCK; TRIM: STAINLESS STEEL; SOFTGOODS: NBR; APPLICATION: WATER; GRADE: 1.4409; SPECIFICATION: EN ISO 5211; STYLE: CENTERED DISC; SCHEDULE: EN 558 SERIES 20; SPECIAL FEATURES: NONE; MANUF P/N: Z011-A; .","PISTER, PAKER ,KLINGER MZANSI, SUPERPUMP,VALVES FOR AFTICA","BUTTERFLY; WAFER","DN 100","CI","10 BAR","STAINLESS STEEL","CENTER FLANGE","52 MM","180 MM","LEVERLOCK","WATER","-40 TO 200 DEG C","Z011-A",null,"NBR"]
["Ingula Pumped Storage Scheme",637555,"VALVE, CHECK: TYPE: NON RETURN; VALVE SIZE: G 3/4 IN; DESIGN RATING: 1 BAR; TEMPERATURE RATING: 0-100 DEG C; CONNECTION: THD; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 76 MM; OPERATED: AIR; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: STAINLESS STEEL; APPLICATION: COMPRESSOR; SPECIFICATION: V592; GRADE: 316; MANUF P/N: RHD20SOMD71; MODEL NO: WP6310; FOR USE ON JP SAUER AND SOHN COMPPRESSOR","PISTER, PAKER ,KLINGER MZANSI, SUPERPUMP,VALVES FOR AFTICA","CHECK; NON RETURN","G 3/4 IN","STAINLESS STEEL","1 BAR","STAINLESS STEEL","THD","76 MM","N/A","AIR","COMPRESSOR; JP SAUER AND SOHN COMPPRESSOR","0-100 DEG C","RHD20SOMD71; WP6310",null,"STAINLESS STEEL"]
["Ingula Pumped Storage Scheme",715945,"VALVE, CHECK: TYPE: NON-RETURN; VALVE SIZE: 650 MM; DESIGN RATING: Y 0.35 AND VACUUM MPA; TEMPERATURE RATING: 200 DEG C; CONNECTION: BUTT-WELDED; BODY MATERIAL: STEEL ASTM A216-WCB; FACE TO FACE LENGTH: 1448 MM; OPERATED: AUTO; TRIM: STEEL; APPLICATION: CHECK VALVE LBS30AA501; SPECIFICATION: ANSI B16 34 CLASS 150; DRAWING NO: FB21EV650NFDA ITEM DEWRANCE; BLED STEAM CHECK VALVE, BODY: WBC, SEAT: CR13, DISK: CR18","Dewrance","CHECK; BODY; NON-RETURN","650 MM","STEEL ASTM A216-WCB","Y 0.35 AND VACUUM MPA","STEEL","BUTT-WELDED","1448 MM","N/A","AUTO","CHECK VALVE LBS30AA501","200 DEG C","FB21EV650NFDA ITEM DEWRANCE",null,"CR13, DISK: CR18"]
["Ingula Pumped Storage Scheme",655823,"VALVE, CHECK: TYPE: PRESSURE; VALVE SIZE: DN400; DESIGN RATING: 16 BAR; TEMPERATURE RATING: -20 TO 200 DEG C; CONNECTION: FLANGED; BODY MATERIAL: CI; FACE TO FACE LENGTH: 480 MM; OPERATED: WATER; STYLE: 1 WAY; TRIM: 315E; SOFTGOODS: STAINLESS STEEL; APPLICATION: VARIOUS; SPECIFICATION: EN558/8; GRADE: GSC25; PERNOW","PERNOW, SUPERPUMP","CHECK; PRESSURE","DN400","CI","16 BAR","315E","FLANGED","480 MM","565 MM","WATER","VARIOUS","-20 TO 200 DEG C",null,null,"STAINLESS STEEL"]
["Ingula Pumped Storage Scheme",623866,"VALVE, SOLENOID: PIPE SIZE: PORT 7.5 MM; STYLE: 3/2; POTENTIAL: 24 VDC; DESIGN RATING: 350 BAR; CONNECTION: FLANGE; BODY MATERIAL: CI; OPERATED: PRESSURE; ENCLOSURE RATING: IP65; MEDIUM: OIL; POWER: 30 W; CURRENT: 1.25 A; APPLICATION: INTAKE EMERGENCY GATE HOIST; OEM P/N: M-3SED6UK13/350CG24N9K4, OEM: BOSCH REXROTH","Bosch; Rexroth","SOLENOID","PORT 7.5 MM","CI","350 BAR",null,"FLANGE",null,null,"PRESSURE","OIL; INTAKE EMERGENCY GATE HOIST",null,"M-3SED6UK13/350CG24N9K4, OEM: BOSCH REXROTH","24 VDC; 30 W; 1.25 A; IP65"]
["Ingula Pumped Storage Scheme",623874,"VALVE, SOLENOID: PIPE SIZE: PORT 11 MM; STYLE: 4 WAY; POTENTIAL: 24 VDC; DESIGN RATING: 350 BAR; CONNECTION: FLANGE; BODY MATERIAL: CI; OPERATED: PRESSURE; ENCLOSURE RATING: IP65; MEDIUM: OIL; POWER: 40 W; CURRENT: 1.61 A; SOFTGOODS: SEALS NBR; APPLICATION: INTAKE HYDRAULIC POWER UNIT; SPECIFICATION: ISO 4401-05-04-0-05; OEM P/N: 4WE10C50/EG24N9K4/M, OEM: BOSCH REXROTH","Bosch; Rexroth","SOLENOID","PORT 11 MM","CI","350 BAR",null,"FLANGE",null,null,"PRESSURE","OIL; INTAKE HYDRAULIC POWER UNIT",null,"4WE10C50/EG24N9K4/M, OEM: BOSCH REXROTH","24 VDC; 40 W; 1.61 A; IP65","SEALS NBR"]
["Ingula Pumped Storage Scheme",726792,"VALVE, SOLENOID: PIPE SIZE: 28 MM; STYLE: COAXIAL 3/2 WAY DIRECT ACTING; POTENTIAL: 230 VAC; DESIGN RATING: 100 BAR; CONNECTION: G3/4 IN FEMALE; BODY MATERIAL: BRASS; OPERATED: SOLENOID; ENCLOSURE RATING: IP65; MEDIUM: AIR; POWER: 0.4 W; CURRENT: 0.15 A; ORIFICE SIZE: 15 MM; SOFTGOODS: NBR ORING; APPLICATION: DRAIN VALVE; MANUF P/N: 039599; STAGE 3 DRAIN VALVE","Coax","SOLENOID","28 MM; 15 MM","BRASS","100 BAR",null,"G3/4 IN FEMALE",null,null,"SOLENOID","AIR; DRAIN VALVE",null,39599,"230 VAC; 0.4 W; 0.15 A; IP65","NBR ORING"]
["Ingula Pumped Storage Scheme",62540,"VALVE, SOLENOID: POTENTIAL: 220 V; SUPPL P/N: S2155",null,"SOLENOID",{"$nulls":10},"S2155","220 V"]
["Ingula Pumped Storage Scheme",668248,"VALVE, SOLENOID: PIPE SIZE: 1-1/2 IN; STYLE: PLUNGER; POTENTIAL: 230 V; DESIGN RATING: 16 BAR; CONNECTION: THREADED; BODY MATERIAL: BRONZE; OPERATED: SOLENOID; ENCLOSURE RATING: NONE; MEDIUM: AIR; POWER: 16 W; CURRENT: 0.07 A; ORIFICE SIZE: 1-1/2 IN; APPLICATION: AUTO DRAIN",null,"SOLENOID","1-1/2 IN","BRONZE","16 BAR",null,"THREADED",null,null,"SOLENOID","AIR; AUTO DRAIN",null,null,"230 V; 16 W; 0.07 A; NONE"]
["Ingula Pumped Storage Scheme",617885,"VALVE, SOLENOID: PIPE SIZE: 1/4 IN; STYLE: 2/1; POTENTIAL: 220 VDC; DESIGN RATING: 2 MPA; CONNECTION: IN; BODY MATERIAL: STEEL; OPERATED: SOLENOID TO OPEN, SPRING TO CLOSE; ENCLOSURE RATING: IP65; MEDIUM: GAS/LIQUID/OIL; POWER: 10 W; CURRENT: 22 A; DRAWING NO: M795-5E4971 REV 0; CAT NO: YS301GH27N9BC7",null,"SOLENOID","1/4 IN","STEEL","2 MPA",null,"IN",null,null,"SOLENOID TO OPEN, SPRING TO CLOSE","GAS/LIQUID/OIL",null,"M795-5E4971 REV 0; YS301GH27N9BC7","220 VDC; 10 W; 22 A; IP65"]
["Ingula Pumped Storage Scheme",668261,"VALVE, SOLENOID: PIPE SIZE: 1 IN; STYLE: PLUNGER; POTENTIAL: 230 V; DESIGN RATING: 33 BAR; CONNECTION: THREADED; BODY MATERIAL: BRONZE; OPERATED: SOLENOID; ENCLOSURE RATING: NONE; MEDIUM: AIR; POWER: 16 W; CURRENT: 0.07 A; ORIFICE SIZE: 1 IN; APPLICATION: AUTO DRAIN",null,"SOLENOID","1 IN","BRONZE","33 BAR",null,"THREADED",null,null,"SOLENOID","AIR; AUTO DRAIN",null,null,"230 V; 16 W; 0.07 A; NONE"]
["Ingula Pumped Storage Scheme",694573,"VALVE, SOLENOID: PIPE SIZE: 1 IN; STYLE: 1/1; POTENTIAL: 24 VDC; DESIGN RATING: 10 BAR; CONNECTION: FNPT; BODY MATERIAL: STAINLESS STEEL; OPERATED: COIL SOLENOID VALVE; ENCLOSURE RATING: IP65; MEDIUM: DIESEL; ORIFICE SIZE: 15-25 MM; COIL: SINGLE; SOFTGOODS: O RING; APPLICATION: DIESEL; MODEL NO 2W-160-15, BOTH VALVE PORT; SIZE 1 IN",null,"SOLENOID","1 IN; 15-25 MM","STAINLESS STEEL","10 BAR",null,"FNPT",null,null,"COIL SOLENOID VALVE","DIESEL",null,"2W-160-15, BOTH VALVE PORT","24 VDC; SINGLE; IP65","O RING"]
["Ingula Pumped Storage Scheme",659669,"VALVE, RELIEF: VALVE SIZE: 1 IN; SET PRESSURE: 0.025-0.08 BAR; TEMPERATURE RATING: -10 TO 100 DEG C; CONNECTION: 1 X 1-1/2 IN; BODY MATERIAL: DIE-CAST AL; TRIM: OT 58 UNI 2012 BRS; FACE TO FACE LENGTH: 90 DEG; OPERATED: SPRING-LOADED; ORIFICE SIZE: 32 MM; SPECIFICATION: ISO 9001; APPLICATION: VARIOUS; STYLE: ONE WAY; SOFTGOODS: BUNA-N; DESIGN RATING: 6 BAR; PRESSURE RANGE: 0-6 BAR; OEM P/N: V/50; TARTARINI","REXROTH","RELIEF","1 IN; 32 MM","DIE-CAST AL","6 BAR; 0-6 BAR; 0.025-0.08 BAR","OT 58 UNI 2012 BRS","1 X 1-1/2 IN","90 DEG","N/A","SPRING-LOADED","VARIOUS","-10 TO 100 DEG C","V/50",null,"BUNA-N"]
["Ingula Pumped Storage Scheme",623862,"VALVE, CHECK: TYPE: FLOW CONTROL; VALVE SIZE: 1-1/4 IN; DESIGN RATING: 320 BAR; TEMPERATURE RATING: -20 TO 100 DEG C; CONNECTION: THD; BODY MATERIAL: STEEL; FACE TO FACE LENGTH: 134.5 MM; OPERATED: PRESSURE, 8 BAR; STYLE: 1 WAY; APPLICATION: SURGE CHAMBER HOIST; SPECIFICATION: EN 10083; OEM P/N: FT257/6 114 8 BAR","PISTER, PAKER ,KLINGER MZANSI, SUPERPUMP,VALVES FOR AFTICA","CHECK; FLOW CONTROL","1-1/4 IN","STEEL","320 BAR","HARDENED STEEL","THD","134.5 MM","N/A","PRESSURE, 8 BAR","SURGE CHAMBER HOIST","-20 TO 100 DEG C","FT257/6 114 8 BAR"]
["Ingula Pumped Storage Scheme",637556,"VALVE, CHECK: TYPE: NON RETURN; VALVE SIZE: 1-5/8 IN; DESIGN RATING: 10 BAR; TEMPERATURE RATING: 0-100 DEG C; CONNECTION: THD; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 118 MM; OPERATED: AIR; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: STAINLESS STEEL; APPLICATION: COMPRESSOR; SPECIFICATION: V592; GRADE: 42/L; MANUF P/N: 036471; MODEL NO: WP6310; FOR USE ON JP SAUER AND SOHN COMPRESSOR.","PERNOW, SUPERPUMP","CHECK; NON RETURN","1-5/8 IN","STAINLESS STEEL","10 BAR","STAINLESS STEEL","THD","118 MM","N/A","AIR","COMPRESSOR; JP SAUER AND SOHN COMPRESSOR","0-100 DEG C","036471; WP6310",null,"STAINLESS STEEL"]
["Ingula Pumped Storage Scheme",637558,"VALVE, CHECK: TYPE: NON RETURN; VALVE SIZE: DIN 50; DESIGN RATING: PN40; TEMPERATURE RATING: 0-100 DEG C; CONNECTION: THD FEMALE; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 150 MM; OPERATED: WATER; STYLE: 2 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: STAINLESS STEEL; APPLICATION: COMPRESSOR; SPECIFICATION: CE0062; GRADE: 1.4408; REFERENCE NO: M410; END ARMATUREN","PERNOW, SUPERPUMP","CHECK; NON RETURN","DIN 50","STAINLESS STEEL","PN40","STAINLESS STEEL","THD FEMALE","150 MM","N/A","WATER","COMPRESSOR","0-100 DEG C","M410",null,"STAINLESS STEEL"]
["Ingula Pumped Storage Scheme",628742,"VALVE, CHECK: TYPE: NON RETURN; VALVE SIZE: DN 100; DESIGN RATING: PN40; TEMPERATURE RATING: -200 TO 550 DEG C; CONNECTION: FLANGE; BODY MATERIAL: CI 300; FACE TO FACE LENGTH: 60 MM; OPERATED: HAND; STYLE: 1 WAY; TRIM: STAINLESS STEEL; APPLICATION: VARIOUS; SPECIFICATION: (PED) 97/23/EC; GRADE: 1.4408; MANUF P/N: RK86A; WITH BODY CENTERING CAMS; FLOWSERVE","Flowserve Gestra","CHECK; NON RETURN","DN 100","CI 300","PN40","STAINLESS STEEL","FLANGE","60 MM","PCD: 190 mm Number of Holes: 8 holesHole Diameter: 22 mm (for M20 bolts)","HAND","VARIOUS","-200 TO 550 DEG C","RK86A"]
["Ingula Pumped Storage Scheme",637559,"VALVE, CHECK: TYPE: NON RETURN; VALVE SIZE: DN 80; DESIGN RATING: PN100-160; TEMPERATURE RATING: 0-100 DEG C; CONNECTION: FLANGE; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 71 MM; OPERATED: WATER; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: STAINLESS STEEL; APPLICATION: COMPRESSOR; SPECIFICATION: CE 0525 05.14; GRADE: 1.4404; MANUF P/N: SR30.160","Gestra","CHECK; NON RETURN","DN 80","STAINLESS STEEL","PN100-160","STAINLESS STEEL","FLANGE","71 MM","Pitch Circle Diameter (PCD): 180 mmNumber of Bolt Holes: 8 holesBolt Hole Diameter: 26 mm (designed for M24 bolts)Flange Outside Diameter (OD): 230 mm","WATER","COMPRESSOR","0-100 DEG C","SR30.160",null,"STAINLESS STEEL"]
["Ingula Pumped Storage Scheme",655829,"VALVE, DIAPHRAGM: TYPE: WET PILOT ACTUATION; VALVE SIZE: 6 IN; DESIGN RATING: 250 PSI; TEMPERATURE RATING: -20 TO 200 DEG C; CONNECTION: FLANGED; BODY MATERIAL: CI; DIAPHRAGM MATERIAL: BUNA; FACE TO FACE LENGTH: 470 MM; OPERATED: PRESSURE; STYLE: 1 WAY; SOFTGOODS: BUNA; APPLICATION: SPRAY WATER; SPECIFICATION: ISO 9001; GRADE: 9YA4; MANUF P/N: DV506FS2","Tyco Fire Protection","DIAPHRAGM; WET PILOT ACTUATION","6 IN","CI; BUNA","250 PSI","BUNA","FLANGED","470 MM","Hole Diameter: 22 mm (for M20 bolts","PRESSURE","SPRAY WATER","-20 TO 200 DEG C","DV506FS2",null,"BUNA"]
["Ingula Pumped Storage Scheme",657954,"VALVE, FLAPPER: TYPE: CHECK; BORE DIAMETER: DN65; CONNECTION: FLANGE; MATERIAL: STAINLESS STEEL; APPLICATION: TURBINE; SPECIFICATION: ISO 9001; MANUF P/N: 5N546CL; PRESSURE RATING: PN100; MATERIAL GRADE: 1.4408","VERVOVALVE,ORION VALVE","FLAPPER; CHECK","DN65","STAINLESS STEEL","PN100 (100 bar = 10 MPa / Approx. 1450 PSI or Class 600)","GX5CrNiMo19-11-2 / Cast 316 Stainless Steel / CF8M","FLANGE","Face-to-Face Dimension: 46 mm (1.81 inches)","Flange Outer Diameter (OD): 205 mmBolt Circle Diameter (PCD): 145 mmBolt Hole Quantity: 8 holesBolt Hole Diameter: 26 mm (Uses M24 size bolts)","Valve Type: Check Valve / Non-Return Valve (Flapper / Swing Type). It operates automatically using line pressure to allow unidirectional fluid flow and prevent dangerous backflow or water hammer. [1, 2, 3, 4, 5]","TURBINE","100°C: 100.0 bar","5N546CL"]
["Ingula Pumped Storage Scheme",657955,"VALVE, FLAPPER: TYPE: CHECK; BORE DIAMETER: DN80; CONNECTION: FLANGE; MATERIAL: STAINLESS STEEL; APPLICATION: TURBINE; SPECIFICATION: ISO 9001; MANUF P/N: 4N602CL; PRESSURE RATING: PN160; MATERIAL GRADE: 1.4408","Velan Inc, Atwood & Morrill (Trillium Flow Technologies),Sempell (Emerson)","FLAPPER; CHECK","DN80 (80mm / approx. 3-inch)","STAINLESS STEEL","PN160 (160 Bar / 16 MPa / approx. 2320 PSI)","Stainless Steel Grade 1.4408 (GX5CrNiMo19-11-2)","FLANGE","46 mm","Bolt Circle Diameter (PCD): 145 mm","IN LINE FLOW CONTROLLED","TURBINE","-196°C up to +400°C","4N602CL"]
["Ingula Pumped Storage Scheme",620393,"VALVE, GATE: VALVE SIZE: 100 MM; TYPE: ISOLATING; CONNECTION: FLANGE; FACE TO FACE LENGTH: 300 MM; BODY MATERIAL: SCS13; TRIM: SS GR 304; OPERATED: HANDWHEEL; STEM DESIGN: RISING; STYLE: 1 WAY; TEMPERATURE RATING: 20 K; APPLICATION: AIR COOLER; DESIGN RATING: JIS 20 K","KITZ Corporation , Shoritsu (Japan) , Bestway Valve (China) , J-Valves Fluid Equipment (China)","GATE; ISOLATING","100 MM","SCS13","JIS 20 K","SS GR 304; RISING","FLANGE","300 MM","Pitch Circle Diameter (PCD): 185 mmNumber of Bolt Holes: 8 holesBolt Hole Diameter: 23 mmRecommended Bolt Size: M20","HANDWHEEL","AIR COOLER","20 K"]
["Ingula Pumped Storage Scheme",620394,"VALVE, GATE: VALVE SIZE: 1-1/2 IN; TYPE: ISOLATING; CONNECTION: FLANGE; FACE TO FACE LENGTH: 160 MM; BODY MATERIAL: A105; TRIM: 13CR; OPERATED: HANDWHEEL; STEM DESIGN: RISING; STYLE: 1 WAY; TEMPERATURE RATING: 840 DEG F; APPLICATION: OIL LEVEL; DESIGN RATING: JIS 10K; .","KITZ Corporation (Japan) , Toyo Valve (Japan) , Hitachi Valves , Velan or Neway","GATE; ISOLATING","1-1/2 IN","A105","JIS 10K","13CR; RISING","FLANGE","160 MM","Pitch Circle Diameter (PCD): 105 mmNumber of Bolt Holes: 4 holesBolt Hole Diameter: 19 mm Recommended Bolt Size: M16","HANDWHEEL","OIL LEVEL","840 DEG F"]
["Ingula Pumped Storage Scheme",620397,"VALVE, GATE: VALVE SIZE: 200 MM; TYPE: ISOLATING; CONNECTION: FLANGE; FACE TO FACE LENGTH: 450 MM; BODY MATERIAL: SCS13; TRIM: SS GR 304; OPERATED: CHAIN, HANDWHEEL; STEM DESIGN: RISING; STYLE: 1 WAY; TEMPERATURE RATING: 20K DEG F; APPLICATION: AIR COOLER; DESIGN RATING: JIS 20 K","KITZ Corporation (Japan): , Tozen Corporation , Shoritsu Seisakusho","GATE; ISOLATING","200 MM","SCS13","JIS 20 K","SS GR 304; RISING","FLANGE","450 MM","Pitch Circle Diameter (PCD): 305 mm Number of Bolt Holes: 12 holesBolt Hole Diameter: 25 mm Recommended Nominal Bolt Size: M22","CHAIN, HANDWHEEL","AIR COOLER","20K DEG F"]
["Ingula Pumped Storage Scheme",620398,"VALVE, GATE: VALVE SIZE: 200 MM; TYPE: ISOLATING; DESIGN PRESSURE: JIS 20 K; DESIGN TEMPERATURE: 20 K; CONNECTION: FLANGE; FACE TO FACE LENGTH: 450 MM; BODY MATERIAL: SCS13; TRIM: SS GR 304; OPERATED: HANDWHEEL; STEM DESIGN: RISING; STYLE: 1 WAY; TEMPERATURE RATING: 20K DEG F; APPLICATION: OIL COOLER; DESIGN RATING: JIS 20K K","KITZ Corporation , Toyo Valve Co., Ltd , Toa Valve Engineering Inc","GATE; ISOLATING","200 MM","SCS13","JIS 20K K; JIS 20 K","SS GR 304; RISING","FLANGE","450 MM","PCD (Pitch Circle Diameter): 305 mm Number of Bolt Holes: 12 holesBolt Hole Diameter: 25 mm (Uses M22 bolts)Flange Outer Diameter (OD): 350 mm","HANDWHEEL","OIL COOLER","20K DEG F; 20 K"]
["Ingula Pumped Storage Scheme",620391,"VALVE, GATE: VALVE SIZE: 250 MM; TYPE: ISOLATING; DESIGN PRESSURE: 2-2.8 MPA; DESIGN TEMPERATURE: 220-350 DEG C; CONNECTION: FLANGE; FACE TO FACE LENGTH: 455 MM; BODY MATERIAL: STAINLESS STEEL; TRIM: HF; OPERATED: ACTUATOR; STEM DESIGN: NON RISING; STYLE: 1 WAY; TEMPERATURE RATING: 20 K; PORT TYPE: STANDARD; APPLICATION: TURBINE; SPECIFICATION: ISO 9001; SPECIAL FEATURES: NONE; GRADE: 304; DESIGN RATING: JIS 20K","KITZ Corporation , Velan Inc. , Kubota Corporation","GATE; ISOLATING; STANDARD","250 MM","STAINLESS STEEL","JIS 20K; 2-2.8 MPA","HF; NON RISING","FLANGE","455 MM","Pitch Circle Diameter (PCD): 380 mm (The center-to-center diameter of the bolt circle)Number of Bolt Holes: 12 holesBolt Hole Diameter: 27 mm (Designed to fit metric M24 flange bolts)","ACTUATOR","TURBINE","20 K; 220-350 DEG C"]
["Ingula Pumped Storage Scheme",655828,"VALVE, DIAPHRAGM: TYPE: WET PILOT ACTUATION; VALVE SIZE: 4 IN; DESIGN RATING: 250 PSI; TEMPERATURE RATING: -20 TO 200 DEG C; CONNECTION: FLANGED; BODY MATERIAL: CI; DIAPHRAGM MATERIAL: BUNA; FACE TO FACE LENGTH: 400 MM; OPERATED: PRESSURE; STYLE: 1 WAY; SOFTGOODS: BUNA; APPLICATION: SPRAY WATER; SPECIFICATION: ISO 9001; GRADE: 9YA4; MANUF P/N: DV504FS2","Tyco Fire Protection Products, a brand under Johnson Controls","DIAPHRAGM; WET PILOT ACTUATION","4 IN","CI; BUNA","250 PSI","BUNA","FLANGED","400 MM","No of holes :8","PRESSURE","SPRAY WATER","-20 TO 200 DEG C","DV504FS2",null,"BUNA"]
["Ingula Pumped Storage Scheme",637405,"VALVE, CHECK: TYPE: RIGHT ANGLE; VALVE SIZE: 3 IN; DESIGN RATING: 21 MPA; TEMPERATURE RATING: -15 TO 75 DEG C; CONNECTION: BOLTED; BODY MATERIAL: STL ALLOY; FACE TO FACE LENGTH: 72.5 X 87 MM; OPERATED: SPRING; MODEL NO: C2G-805-S3","Tokyo Keiki Inc. / TOKIMEC","CHECK; RIGHT ANGLE","3 IN","STL ALLOY","21 MPA","Alloy Steel.","BOLTED","72.5 X 87 MM","Bolt Hole Diameter: 27 mm (Designed to fit metric M24 flange bolts","SPRING","STANDARD INDUSTRIAL USE","-15 TO 75 DEG C","C2G-805-S3"]
["Ingula Pumped Storage Scheme",721178,"VALVE, CHECK: TYPE: TL34; VALVE SIZE: 3 IN; DESIGN RATING: 2 BAR; TEMPERATURE RATING: -40-100 DEG C; CONNECTION: DN 80, 3 IN PIPE; BODY MATERIAL: ALSI7MG0.65T685HBS; FACE TO FACE LENGTH: 1.00 M; OPERATED: 250 VDC SUPPLY; TL34 CONSERVATOR SHUTTER VALVE; MAXIMUM SWITCHING, VOLTAGE 250 VDC; BODY MATERIAL: ALSI7MG0.6ST685 HBS; 3 IN; SIZE: DN80; SERGI (FRANCE)","SERGI","CHECK; TL34","3 IN","ALSI7MG0.65T685HBS; ALSI7MG0.6ST685 HBS","2 BAR","STAINLESS STEEL","DN 80, 3 IN PIPE","1.00 M","160 MM","250 VDC SUPPLY","TRANSFORMER OIL ","-40-100 DEG C"]
["Ingula Pumped Storage Scheme",731175,"VALVE, CHECK: TYPE: TL34; VALVE SIZE: DN80; DESIGN RATING: 2 BAR; TEMPERATURE RATING: -40 to 100 DEG C; CONNECTION: SIZE 0 GLAND; BODY MATERIAL: CAST IRON; FACE TO FACE LENGTH: 210.5 MM; OPERATED: 220VDC","KLINGER,SUPERPUMP","CHECK; TL34","DN80","CAST IRON","2 BAR","STAINLESS STEEL","SIZE 0 GLAND","210.5 MM","160 MM","220VDC","TRANSFORMER OIL SYSTEMS, COMPRESSORS","-40 to 100 DEG C"]
["Ingula Pumped Storage Scheme",635725,"VALVE, CHECK: TYPE: WAFER; VALVE SIZE: DN65; DESIGN RATING: 20 BAR; TEMPERATURE RATING: 0-120 DEG C; CONNECTION: FLANGE; BODY MATERIAL: GGG40; FACE TO FACE LENGTH: 46 MM; OPERATED: FLOW; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: EPDM; APPLICATION: CHILLER; GRADE: 1.4401; MANUF P/N: 915S25/1/E; DUAL WAFER","KLINGER,SUPERPUMP","CHECK; WAFER","DN65","GGG40","20 BAR","STAINLESS STEEL","FLANGE","46 MM","N/A","FLOW","CHILLER","0-120 DEG C","915S25/1/E",null,"EPDM"]
["Ingula Pumped Storage Scheme",623867,"VALVE, CHECK: TYPE: SUBPLATE; VALVE SIZE: NS10; DESIGN RATING: 350 BAR; TEMPERATURE RATING: -20 TO 80 DEG C; CONNECTION: FLANGE; BODY MATERIAL: CI; FACE TO FACE LENGTH: 50 MM; OPERATED: OIL PRESSURE; STYLE: 1/1; SOFTGOODS: FKM; APPLICATION: INTAKE HYDRAULIC POWER UNIT; SPECIFICATION: DIN 51524; OEM P/N: Z1S10B05-2-41/F, OEM: BOSCH REXROTH","Bosch; Rexroth","CHECK; SUBPLATE","NS10","CI","350 BAR","HARDENED STEEL, SPRING STEEL","FLANGE","50 MM","N/A","OIL PRESSURE","INTAKE HYDRAULIC POWER UNIT","-20 TO 80 DEG C","Z1S10B05-2-41/F, OEM: BOSCH REXROTH",null,"FKM"]
["Ingula Pumped Storage Scheme",623870,"VALVE, CHECK: TYPE: TWIN THROTTLE; VALVE SIZE: NS6; DESIGN RATING: 315 BAR; TEMPERATURE RATING: -20 TO 80 DEG C; CONNECTION: FLANGE; BODY MATERIAL: CI; FACE TO FACE LENGTH: 40 MM; OPERATED: OIL PRESSURE; SOFTGOODS: SEALS FKM; APPLICATION: INTAKE HYDRAULIC POWER UNIT; SPECIFICATION: DIN 51524; OEM P/N: Z2FS6-2-44/2QV, OEM: BOSCH REXROTH; .","Bosch; Rexroth","CHECK; TWIN THROTTLE","NS6","CI","315 BAR","HARDENED STEEL","FLANGE","40 MM","N/A","OIL PRESSURE","INTAKE HYDRAULIC POWER UNIT","-20 TO 80 DEG C","Z2FS6-2-44/2QV, OEM: BOSCH REXROTH",null,"SEALS FKM"]
["Ingula Pumped Storage Scheme",620183,"VALVE, GLOBE: VALVE SIZE: 1/2 IN; DESIGN PRESSURE: 2.0 MPA; DESIGN TEMPERATURE: <100 DEG C; FACE TO FACE LENGTH: 150 MM; OPERATED: HANDWHEEL; CONNECTION: FLANGED; BODY MATERIAL: F304; TRIM: SS GR 304/STL; GRADE: ASTM A182 F304; SOFTGOODS: NEOPRENE; STEM DESIGN: RISING SPINDLE; STYLE: DIRECTIONAL; APPLICATION: DRAIN AIR/OIL COOLER; SPECIFICATION: ISO9001; TYPE: SHUT OFF; DESIGN RATING: JIS 20K; S AND S VALVE","VALVE FOR AFRICA ,SUPERPUMP, KLINGER MZANSI","GLOBE; SHUT OFF","1/2 IN","F304","JIS 20K; 2.0 MPA","SS GR 304/STL; RISING SPINDLE","FLANGED","150 MM","70 MM","HANDWHEEL","DRAIN AIR/OIL COOLER","<100 DEG C",null,null,"NEOPRENE"]
["Ingula Pumped Storage Scheme",64665,"VALVE, GLOBE: VALVE SIZE: 15 MM; OPERATED: MANUAL; CONNECTION: SW; BODY MATERIAL: CS; DESIGN RATING: 600 LB; MANUF P/N: SASSWJ0015BR","VALVE FOR AFRICA ,SUPERPUMP, KLINGER MZANSI","GLOBE","15 MM","CS","600 LB","STELLITE, STAINLESS STEEL","SW","110 - 140 MM","N/A","MANUAL","WATER, OIL, AIR","–20°C to 100°C","SASSWJ0015BR"]
["Ingula Pumped Storage Scheme",620408,"VALVE, GLOBE: VALVE SIZE: 2 IN; FACE TO FACE LENGTH: 200 MM; OPERATED: HANDWHEEL; CONNECTION: FLANGE; BODY MATERIAL: A105; TRIM: 13CR; STEM DESIGN: RISING; STYLE: 1 WAY; APPLICATION: DRAIN; TYPE: ISOLATING; DESIGN RATING: JIS 10K; TEMPERATURE RATING: 840 DEG F","PAKER, SUPERPUMP , HYDRAULICS, PISTER","GLOBE; ISOLATING","2 IN","A105","JIS 10K","13CR; RISING","FLANGE","200 MM","120 MM","HANDWHEEL","DRAIN","840 DEG F"]
["Ingula Pumped Storage Scheme",620407,"VALVE, GLOBE: VALVE SIZE: 50 MM; FACE TO FACE LENGTH: 200 MM; OPERATED: HANDWHEEL; CONNECTION: FLANGE; BODY MATERIAL: SCS13; TRIM: SS GR 304; STEM DESIGN: RISING; STYLE: 1 WAY; APPLICATION: DRAIN; TYPE: ISOLATING; DESIGN RATING: JIS 20K; TEMPERATURE RATING: 20K","PAKER, SUPERPUMP , HYDRAULICS, PISTER","GLOBE; ISOLATING","50 MM","SCS13","JIS 20K","SS GR 304; RISING","FLANGE","200 MM","120 MM","HANDWHEEL","DRAIN","20K"]
["Ingula Pumped Storage Scheme",620181,"VALVE, GLOBE: VALVE SIZE: 1/2 IN; DESIGN PRESSURE: 1 TO 1.2 MPA; DESIGN TEMPERATURE: 220 TO 300 DEG C; FACE TO FACE LENGTH: 105 MM; OPERATED: HANDWHEEL; CONNECTION: FLANGED; BODY MATERIAL: A105; TRIM: STL 13CR; GRADE: ASTM A105; SOFTGOODS: NEOPRENE; STEM DESIGN: RISING SPINDLE; STYLE: DIRECTIONAL; APPLICATION: OIL DRAIN; SPECIFICATION: ISO 9001; TYPE: SHUT OFF; DESIGN RATING: JIS 10K; TEMPERATURE RATING: 100 DEG F; OEM P/N: SC-F10K-15A; S AND S VALVE","PAKER, SUPERPUMP , HYDRAULICS, PISTER,","GLOBE; SHUT OFF","1/2 IN","A105","JIS 10K; 1 TO 1.2 MPA","STL 13CR; RISING SPINDLE","FLANGED","105 MM","70 MM","HANDWHEEL","OIL DRAIN","100 DEG F; 220 TO 300 DEG C","SC-F10K-15A",null,"NEOPRENE"]
["Ingula Pumped Storage Scheme",620186,"VALVE, GLOBE: VALVE SIZE: 1 IN; DESIGN PRESSURE: 1 TO 1.2 MPA; DESIGN TEMPERATURE: 220 TO 300 DEG C; FACE TO FACE LENGTH: 125 MM; OPERATED: HANDWHEEL; CONNECTION: FLANGED; BODY MATERIAL: A105; TRIM: 13CR/STL; GRADE: ASTM A105; SOFTGOODS: NEOPRENE; STEM DESIGN: RISING SPINDLE; STYLE: DIRECTIONAL; APPLICATION: DRAIN; SPECIFICATION: ISO 9001; TYPE: SHUT OFF; DESIGN RATING: JIS 10K; TEMPERATURE RATING: 840 DEG F; OEM P/N: SC-F10K-25A; S AND S VALVE","PAKER, SUPERPUMP , HYDRAULICS, PISTER","GLOBE; SHUT OFF","1 IN","A105","JIS 10K; 1 TO 1.2 MPA","13CR/STL; RISING SPINDLE","FLANGED","125 MM","90 MM","HANDWHEEL","DRAIN","840 DEG F; 220 TO 300 DEG C","SC-F10K-25A",null,"NEOPRENE"]
["Ingula Pumped Storage Scheme",623904,"VALVE, RELIEF: VALVE SIZE: NS40; SET PRESSURE: ADJUSTABLE; TEMPERATURE RATING: -20 TO 80 DEG C; CONNECTION: FLANGE; BODY MATERIAL: CAST IRON; TRIM: CAST IRON; FACE TO FACE LENGTH: 100 MM; OPERATED: OIL PRESSURE; ORIFICE SIZE: DIA 1.18 MM; SPECIFICATION: DIN 24340; APPLICATION: DRAFT TUBE GATE HOIST; STYLE: 2 WAY; DESIGN RATING: 420 BAR; PRESSURE RANGE: 0-420 BAR; OEM P/N: LFA40H2-71/F, OEM: BOSCH REXROTH; TO BE SUPPLIED WITH VALVE CARTRIDGE LC 40 A05E7X R900937996","Bosch; Rexroth","RELIEF","NS40; DIA 1.18 MM","CAST IRON","420 BAR; 0-420 BAR; ADJUSTABLE","CAST IRON","FLANGE","100 MM","N/A","OIL PRESSURE","DRAFT TUBE GATE HOIST","-20 TO 80 DEG C","LFA40H2-71/F, OEM: BOSCH REXROTH"]
["Ingula Pumped Storage Scheme",623903,"VALVE, RELIEF: VALVE SIZE: NS16; SET PRESSURE: ADJUSTABLE; TEMPERATURE RATING: -20 TO 80 DEG C; CONNECTION: FLANGE; BODY MATERIAL: CAST IRON; TRIM: CAST IRON; FACE TO FACE LENGTH: 35 MM; OPERATED: OIL PRESSURE; ORIFICE SIZE: DIA 0.669 MM; SPECIFICATION: DIN 24340; APPLICATION: DRAFT TUBE GATE HOIST; STYLE: 2 WAY; DESIGN RATING: 420 BAR; PRESSURE RANGE: 0-420 BAR; OEM P/N: LFA16H2-71/F, OEM: BOSCH REXROTH; TO BE SUPPLIED WITH VALVE CARTRIDGE LC 16 A05E7X R900912566","Bosch; Rexroth","RELIEF","NS16; DIA 0.669 MM","CAST IRON","420 BAR; 0-420 BAR; ADJUSTABLE","CAST IRON","FLANGE","35 MM","N/A","OIL PRESSURE","DRAFT TUBE GATE HOIST","-20 TO 80 DEG C","LFA16H2-71/F, OEM: BOSCH REXROTH"]
["Ingula Pumped Storage Scheme",655228,"VALVE, RELIEF: VALVE SIZE: G1/2 IN; SET PRESSURE: 365 KPA; TEMPERATURE RATING: -10 TO 220 DEG C; CONNECTION: G1/2 IN; BODY MATERIAL: 1.4104 (430); TRIM: METAL; FACE TO FACE LENGTH: 46 MM; OPERATED: PRESSURE; ORIFICE SIZE: 10 MM; SPECIFICATION: DIN ISO 228-1; APPLICATION: VARIOUS; GRADE: 1.4104; STYLE: 1 WAY; SOFTGOODS: 1.4404; DESIGN RATING: PN160-400; PRESSURE RANGE: 180-365 BAR; MANUF P/N: 4373.2602; REFERENCE NO: D0 10-D/G 0.5 F 0.35; .","REXROTH","RELIEF","G1/2 IN; 10 MM","1.4104 (430)","PN160-400; 180-365 BAR; 365 KPA","METAL","G1/2 IN","46 MM","N/A","PRESSURE","VARIOUS","-10 TO 220 DEG C","4373.2602; D0 10-D/G 0.5 F 0.35",null,1.4404]
["Ingula Pumped Storage Scheme",639776,"VALVE, RELIEF: VALVE SIZE: G1/2 IN; SET PRESSURE: 3 BAR; TEMPERATURE RATING: 0-20 DEG C; CONNECTION: G1/2 IN; BODY MATERIAL: SS GR 316L; TRIM: SS GR 316L; FACE TO FACE LENGTH: 90 DEG; OPERATED: PRESSURE; ORIFICE SIZE: 1/2 IN; APPLICATION: VARIOUS; GRADE: 1.4404; STYLE: 1 WAY; SOFTGOODS: STAINLESS STEEL; DESIGN RATING: INLET PN250; OUTLET PN160; PRESSURE RANGE: 0-250 BAR; REFERENCE NO: 4374.3144","REXROTH","RELIEF","G1/2 IN; 1/2 IN","SS GR 316L","INLET PN250; 0-250 BAR; 3 BAR","SS GR 316L","G1/2 IN","90 DEG","N/A","PRESSURE","VARIOUS","0-20 DEG C",4374.3144,null,"STAINLESS STEEL"]
["Ingula Pumped Storage Scheme",620399,"VALVE, GATE: VALVE SIZE: 250 MM; TYPE: ISOLATING; CONNECTION: FLANGE; FACE TO FACE LENGTH: 450 MM; BODY MATERIAL: SCS13; TRIM: SS GR 304; OPERATED: CHAIN, HANDWHEEL; STEM DESIGN: RISING; STYLE: 1 WAY; TEMPERATURE RATING: 20K DEG F; APPLICATION: COOLER; DESIGN RATING: JIS 20K; .","PAKER, SUPERPUMP , HYDRAULICS, PISTER","GATE; ISOLATING","250 MM","SCS13","JIS 20K","SS GR 304; RISING","FLANGE","450 MM","370 MM","CHAIN, HANDWHEEL","COOLER","20K DEG F"]
["Ingula Pumped Storage Scheme",620395,"VALVE, GATE: VALVE SIZE: 300 MM; TYPE: ISOLATING; CONNECTION: FLANGE; FACE TO FACE LENGTH: 500 MM; BODY MATERIAL: SCS13; TRIM: SS GR 304; OPERATED: CHAIN, HANDWHEEL; STEM DESIGN: RISING; STYLE: 1 WAY; TEMPERATURE RATING: 20K DEG F; APPLICATION: AIR COOLER; DESIGN RATING: JIS 20K; .","PAKER, SUPERPUMP , HYDRAULICS, PISTER","GATE; ISOLATING","300 MM","SCS13","JIS 20K","SS GR 304; RISING","FLANGE","500 MM","430 MM","CHAIN, HANDWHEEL","AIR COOLER","20K DEG F"]
["Ingula Pumped Storage Scheme",620396,"VALVE, GATE: VALVE SIZE: 300 MM; TYPE: ISOLATING; DESIGN PRESSURE: JIS 20 K; DESIGN TEMPERATURE: 20 K; CONNECTION: FLANGE; FACE TO FACE LENGTH: 500 MM; BODY MATERIAL: SCS13; TRIM: SS GR 304; OPERATED: HANDWHEEL; STEM DESIGN: RISING; STYLE: 1 WAY; TEMPERATURE RATING: 20K DEG F; APPLICATION: OIL COOLER; DESIGN RATING: JIS 20 K","ENERGY VALVES,KLINGER VALVES, FLUID HAUS,SUPERPUMP","GATE; ISOLATING","300 MM","SCS13","JIS 20 K","SS GR 304; RISING","FLANGE","500 MM","430 MM","HANDWHEEL","OIL COOLER","20K DEG F; 20 K"]
["Ingula Pumped Storage Scheme",620392,"VALVE, GATE: VALVE SIZE: 50 MM; TYPE: ISOLATING; CONNECTION: FLANGE; FACE TO FACE LENGTH: 213 MM; BODY MATERIAL: SCS13; TRIM: SS GR 304; OPERATED: HANDWHEEL; STEM DESIGN: RISING; STYLE: 1 WAY; TEMPERATURE RATING: 20K K; APPLICATION: UPPER OIL COOLER; DESIGN RATING: JIS 20K K","ENERGY VALVES,KLINGER VALVES, FLUID HAUS,SUPERPUMP","GATE; ISOLATING","50 MM","SCS13","JIS 20K K","SS GR 304; RISING","FLANGE","213 MM",null,"HANDWHEEL","UPPER OIL COOLER","20K K"]
["Ingula Pumped Storage Scheme",628697,"VALVE, RELIEF: VALVE SIZE: 3/4 IN; SET PRESSURE: 47.2 BAR; TEMPERATURE RATING: -10 TO 100 DEG C; CONNECTION: THREADED FEMALE; BODY MATERIAL: BRASS; TRIM: BRASS; FACE TO FACE LENGTH: 118 MM; OPERATED: PRESSURE; ORIFICE SIZE: 10 MM; SPECIFICATION: ISO 4126-1; APPLICATION: VARIOUS; STYLE: 1 WAY; SOFTGOODS: BRASS; DESIGN RATING: 150 BAR; PRESSURE RANGE: 42-25 BAR; MANUF P/N: H10N11787","REXROTH","RELIEF","3/4 IN; 10 MM","BRASS","150 BAR; 42-25 BAR; 47.2 BAR","BRASS","THREADED FEMALE","118 MM","N/A","PRESSURE","VARIOUS","-10 TO 100 DEG C","H10N11787",null,"BRASS"]
["Ingula Pumped Storage Scheme",637561,"VALVE, RELIEF: VALVE SIZE: DN 3/4 X 1 IN; SET PRESSURE: 53 BAR; TEMPERATURE RATING: -20 TO 200 DEG C; CONNECTION: THD; BODY MATERIAL: BRASS; TRIM: BRASS; FACE TO FACE LENGTH: L SHAPE; OPERATED: AIR; ORIFICE SIZE: 1/2 IN; SPECIFICATION: CE 0035 2011; APPLICATION: COMPRESSOR; GRADE: G14/S; STYLE: 1 WAY; SOFTGOODS: BRASS; MANUF P/N: CW614N","REXROTH","RELIEF","DN 3/4 X 1 IN; 1/2 IN","BRASS","53 BAR","BRASS","THD","L SHAPE","N/A","AIR","COMPRESSOR","-20 TO 200 DEG C","CW614N",null,"BRASS"]
["Ingula Pumped Storage Scheme",655227,"VALVE, RELIEF: VALVE SIZE: DN 1 X 1-1/4 IN; SET PRESSURE: 8 BAR; TEMPERATURE RATING: -20 TO 200 DEG C; CONNECTION: THD; BODY MATERIAL: BRZ; TRIM: BRZ; FACE TO FACE LENGTH: L SHAPE; OPERATED: PRESSURE; ORIFICE SIZE: 1/2 IN; SPECIFICATION: CE0036 2017; APPLICATION: COMPRESSOR; GRADE: G20/S; STYLE: 1 WAY; SOFTGOODS: BRZ; MANUF P/N: 017450016","REXROTH","RELIEF","DN 1 X 1-1/4 IN; 1/2 IN","BRZ","8 BAR","BRZ","THD","L SHAPE","N/A","PRESSURE","COMPRESSOR","-20 TO 200 DEG C",17450016,null,"BRZ"]
["Ingula Pumped Storage Scheme",623863,"VALVE, RELIEF: VALVE SIZE: NS10; SET PRESSURE: ADJUSTABLE; TEMPERATURE RATING: 100 DEG C; CONNECTION: FLANGE; BODY MATERIAL: CAST IRON; TRIM: CAST IRON; FACE TO FACE LENGTH: 30 MM; OPERATED: PILOT; ORIFICE SIZE: ADJUSTABLE; SPECIFICATION: 97/23/EC; APPLICATION: SURGE CHAMBER HOIST; STYLE: 1 WAY; SOFTGOODS: O-RING; DESIGN RATING: 200 BAR; PRESSURE RANGE: 0-200 BAR; OEM P/N: DBW10B2-52/300-6EG24N9K4, OEM: BOSCH REXROTH; WITH BUILT-ON DIRECTIONAL VALVE","Bosch; Rexroth","RELIEF","NS10; ADJUSTABLE","CAST IRON","200 BAR; 0-200 BAR; ADJUSTABLE","CAST IRON","FLANGE","30 MM","N/A","PILOT","SURGE CHAMBER HOIST","100 DEG C","DBW10B2-52/300-6EG24N9K4, OEM: BOSCH REXROTH",null,"O-RING"]
["Ingula Pumped Storage Scheme",644952,"VALVE, RELIEF: VALVE SIZE: 30 MM; SET PRESSURE: 100 BAR; TEMPERATURE RATING: -30 TO 80 DEG C; CONNECTION: SUBPLATE; BODY MATERIAL: STEEL; TRIM: METAL; FACE TO FACE LENGTH: 80 MM; OPERATED: PRESSURE; ORIFICE SIZE: 15 MM; SPECIFICATION: ISO 9001; APPLICATION: VARIOUS; GRADE: 913000149; STYLE: 1 WAY; SOFTGOODS: NBR; DESIGN RATING: 25-400 BAR; PRESSURE RANGE: 0-350 BAR; MANUF P/N: R900423712; MODEL NO: DBDS 30 P1A/100","REXROTH","RELIEF","30 MM; 15 MM","STEEL","25-400 BAR; 0-350 BAR; 100 BAR","METAL","SUBPLATE","80 MM","N/A","PRESSURE","VARIOUS","-30 TO 80 DEG C","R900423712; DBDS 30 P1A/100",null,"NBR"]
["Ingula Pumped Storage Scheme",68148,"VALVE, RELIEF: VALVE SIZE: 50 MM; SET PRESSURE: 35 KPA; CONNECTION: THD; BODY MATERIAL: STL; TRIM: BRASS; OPERATED: SPRING; PRESSURE RANGE: 2-20 LB; REFERENCE NO: MD0014; SAFETY; TYPE 616-2; TYPE: HLP","REXROTH","RELIEF; HLP","50 MM","STL","2-20 LB; 35 KPA","BRASS","THD","N/A","N/A","SPRING","AIR, WATER, OIL, NON-CORROSIVE GASES","–20°C to ~120°C","MD0014"]
["Ingula Pumped Storage Scheme",619974,"VALVE, RELIEF: VALVE SIZE: 1/2 IN; SET PRESSURE: 1.5 MPA; TEMPERATURE RATING: 120 DEG C; CONNECTION: BSP SCREW; BODY MATERIAL: STEEL; TRIM: STEEL; FACE TO FACE LENGTH: T-TYPE; OPERATED: PRESSURE; APPLICATION: PRESSURE REDUCER; DESIGN RATING: 1.5 MPA; PRESSURE RANGE: 1.3-1.5 MPA; REFERENCE NO: ESV-903M","REXROTH","RELIEF","1/2 IN","STEEL","1.5 MPA; 1.3-1.5 MPA","STEEL","BSP SCREW","T-TYPE","N/A","PRESSURE","PRESSURE REDUCER","120 DEG C","ESV-903M"]
["Ingula Pumped Storage Scheme",623857,"VALVE, RELIEF: VALVE SIZE: 1 IN; SET PRESSURE: 94 BAR; TEMPERATURE RATING: 100 DEG C; CONNECTION: FLANGE; BODY MATERIAL: CAST IRON; TRIM: CAST IRON; FACE TO FACE LENGTH: 26 MM; OPERATED: PILOT; ORIFICE SIZE: ADJUSTABLE; SPECIFICATION: ANSI B16.10; APPLICATION: SURGE CHAMBER HOIST; STYLE: 3/2; SOFTGOODS: O-RING; DESIGN RATING: 315 BAR; PRESSURE RANGE: 0-315 BAR; OEM P/N: DB20-2-52/315, OEM: BOSCH REXROTH","Bosch; Rexroth","RELIEF","1 IN; ADJUSTABLE","CAST IRON","315 BAR; 0-315 BAR; 94 BAR","CAST IRON","FLANGE","26 MM","N/A","PILOT","SURGE CHAMBER HOIST","100 DEG C","DB20-2-52/315, OEM: BOSCH REXROTH",null,"O-RING"]
["Ingula Pumped Storage Scheme",660516,"VALVE, PILOT: VALVE STYLE: 1 WAY; VALVE SIZE: 6 MM; MATERIAL: STL; OEM P/N: GPFX730094P0001, OEM: ABB POWER GENERATION (PTY) LTD; MODEL NO: HECPS-3S/5S; 220-250 VDC; FOR USE ON GEN CIRCUIT BREAKER; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",null,"PILOT","6 MM","STL",{"$nulls":6},"GEN CIRCUIT BREAKER",null,"GPFX730094P0001, OEM: ABB POWER GENERATION (PTY) LTD; HECPS-3S/5S"]
["Ingula Pumped Storage Scheme",659664,"VALVE, RELIEF: VALVE SIZE: 8 MM; SET PRESSURE: 11 BAR; TEMPERATURE RATING: -20 TO 200 DEG C; CONNECTION: R1/2 IN; BODY MATERIAL: BRASS; TRIM: STEEL; FACE TO FACE LENGTH: CASCADE; OPERATED: PRESSURE; ORIFICE SIZE: 6 MM; SPECIFICATION: EN 4126-1; APPLICATION: VARIOUS; STYLE: ONE WAY; SOFTGOODS: BRASS; DESIGN RATING: 15 BAR; PRESSURE RANGE: 0.73-15 BAR; OEM P/N: 03/16-08711; BOGE COMPRESSED AIR SYSTEMS","REXROTH,VOITH","RELIEF","8 MM; 6 MM","BRASS","15 BAR; 0.73-15 BAR; 11 BAR","STEEL","R1/2 IN","CASCADE","N/A","PRESSURE","VARIOUS","-20 TO 200 DEG C","03/16-08711",null,"BRASS"]
["Ingula Pumped Storage Scheme",637560,"VALVE, RELIEF: VALVE SIZE: 1 IN; SET PRESSURE: 88 BAR; TEMPERATURE RATING: 0-50 DEG C; CONNECTION: G1 IN-BSPP; BODY MATERIAL: STAINLESS STEEL; TRIM: STAINLESS STEEL; FACE TO FACE LENGTH: L SHAPE; OPERATED: AIR; ORIFICE SIZE: 1 IN; SPECIFICATION: GL1238640; APPLICATION: COMPRESSOR; GRADE: 316; STYLE: 1 WAY; SOFTGOODS: STAINLESS STEEL; DESIGN RATING: 88 BAR G; PRESSURE RANGE: IN PN 250; OUT PN 40; MANUF P/N: M33H03X00V56V66J23H01","REXROTH,VOITH","RELIEF","1 IN","STAINLESS STEEL","88 BAR G; IN PN 250; 88 BAR","STAINLESS STEEL","G1 IN-BSPP","L SHAPE","N/A","AIR","COMPRESSOR","0-50 DEG C","M33H03X00V56V66J23H01",null,"STAINLESS STEEL"]
["Ingula Pumped Storage Scheme",617883,"VALVE, RELIEF: VALVE SIZE: 1/2 IN; SET PRESSURE: 2.1 MPA; TEMPERATURE RATING: 220 DEG C; CONNECTION: 1/2 IN-BSP; BODY MATERIAL: STEEL; TRIM: VARIOUS; FACE TO FACE LENGTH: 110 MM; OPERATED: PRESSURE; APPLICATION: AIR LINES; DESIGN RATING: 2.1 MPA; PRESSURE RANGE: 0-2.1 MPA; DRAWING NO: M705-5A7443A REV 0","REXROTH,VOITH","RELIEF","1/2 IN","STEEL","2.1 MPA; 0-2.1 MPA","VARIOUS","1/2 IN-BSP","110 MM","N/A","PRESSURE","AIR LINES","220 DEG C","M705-5A7443A REV 0"]
["Ingula Pumped Storage Scheme",637562,"VALVE, RELIEF: VALVE SIZE: 1/2 IN; SET PRESSURE: 3 BAR; TEMPERATURE RATING: 0-20 DEG C; CONNECTION: THD 1/2 IN; BODY MATERIAL: STAINLESS STEEL; TRIM: STAINLESS STEEL; FACE TO FACE LENGTH: L SHAPE; OPERATED: AIR; ORIFICE SIZE: 1 IN; SPECIFICATION: 14/980; APPLICATION: COMPRESSOR; GRADE: 316; STYLE: 1 WAY; SOFTGOODS: STAINLESS STEEL; DESIGN RATING: 3 BAR; PRESSURE RANGE: IN PN 250; OUT PN 160; MANUF P/N: M33H03X00V54V65; .","REXROTH,VOITH","RELIEF","1/2 IN; 1 IN","STAINLESS STEEL","3 BAR; IN PN 250","STAINLESS STEEL","THD 1/2 IN","L SHAPE","N/A","AIR","COMPRESSOR","0-20 DEG C","M33H03X00V54V65",null,"STAINLESS STEEL"]
["Ingula Pumped Storage Scheme",644950,"VALVE, RELIEF: VALVE SIZE: 10 MM; SET PRESSURE: 130 BAR; TEMPERATURE RATING: -30 TO 80 DEG C; CONNECTION: THREADED; BODY MATERIAL: STEEL; TRIM: METAL; FACE TO FACE LENGTH: 80 MM; OPERATED: PRESSURE; ORIFICE SIZE: 5 MM; SPECIFICATION: ISO 9001; APPLICATION: VARIOUS; GRADE: 913000149; STYLE: 1 WAY; SOFTGOODS: NBR; DESIGN RATING: 25-400 BAR; PRESSURE RANGE: 0-630 BAR; MANUF P/N: R900778044; MODEL NO: DBDS 10 G19/130E","REXROTH,VOITH","RELIEF","10 MM; 5 MM","STEEL","25-400 BAR; 0-630 BAR; 130 BAR","METAL","THREADED","80 MM","N/A","PRESSURE","VARIOUS","-30 TO 80 DEG C","R900778044; DBDS 10 G19/130E",null,"NBR"]
["Ingula Pumped Storage Scheme",644949,"VALVE, RELIEF: VALVE SIZE: 10 MM; SET PRESSURE: 65 BAR; TEMPERATURE RATING: -30 TO 80 DEG C; CONNECTION: THREADED; BODY MATERIAL: STEEL; TRIM: METAL; FACE TO FACE LENGTH: 80 MM; OPERATED: PRESSURE; ORIFICE SIZE: 5 MM; SPECIFICATION: ISO 9001; APPLICATION: VARIOUS; GRADE: 913000149; STYLE: 1 WAY; SOFTGOODS: NBR; DESIGN RATING: 25-400 BAR; PRESSURE RANGE: 0-630 BAR; MANUF P/N: R901260712; MODEL NO: DBDS 10 G19/65E","REXROTH,VOITH","RELIEF","10 MM; 5 MM","STEEL","25-400 BAR; 0-630 BAR; 65 BAR","METAL","THREADED","80 MM","N/A","PRESSURE","VARIOUS","-30 TO 80 DEG C","R901260712; DBDS 10 G19/65E",null,"NBR"]
["Ingula Pumped Storage Scheme",644951,"VALVE, RELIEF: VALVE SIZE: 30 MM; SET PRESSURE: 130 BAR; TEMPERATURE RATING: -30 TO 80 DEG C; CONNECTION: SUBPLATE; BODY MATERIAL: STEEL; TRIM: METAL; FACE TO FACE LENGTH: 80 MM; OPERATED: PRESSURE; ORIFICE SIZE: 15 MM; SPECIFICATION: ISO 9001; APPLICATION: VARIOUS; GRADE: 913000149; STYLE: 1 WAY; SOFTGOODS: NBR; DESIGN RATING: 25-400 BAR; PRESSURE RANGE: 0-350 BAR; MANUF P/N: R901341824; MODEL NO: DBDS 30 G1A/130E","REXROTH,VOITH","RELIEF","30 MM; 15 MM","STEEL","25-400 BAR; 0-350 BAR; 130 BAR","METAL","SUBPLATE","80 MM","N/A","PRESSURE","VARIOUS","-30 TO 80 DEG C","R901341824; DBDS 30 G1A/130E",null,"NBR"]
["Ingula Pumped Storage Scheme",644953,"VALVE, RELIEF: VALVE SIZE: 20 MM; SET PRESSURE: 100 BAR; TEMPERATURE RATING: -30 TO 80 DEG C; CONNECTION: SUBPLATE; BODY MATERIAL: STEEL; TRIM: METAL; FACE TO FACE LENGTH: NIL; OPERATED: PRESSURE; ORIFICE SIZE: 10 MM; SPECIFICATION: ISO 9001; APPLICATION: VARIOUS; GRADE: 913000149; STYLE: 1 WAY; SOFTGOODS: NBR; DESIGN RATING: 25-400 BAR; PRESSURE RANGE: 10-350 BAR; MANUF P/N: R900597283; MODEL NO: DR 20-5-52/100YM","REXROTH, VOITH","RELIEF","20 MM; 10 MM","STEEL","25-400 BAR; 10-350 BAR; 100 BAR","METAL","SUBPLATE","NIL","N/A","PRESSURE","VARIOUS","-30 TO 80 DEG C","R900597283; DR 20-5-52/100YM",null,"NBR"]
["Ingula Pumped Storage Scheme",637402,"VALVE, RELIEF: VALVE SIZE: 3 IN; SET PRESSURE: 25 MPA; TEMPERATURE RATING: -15 TO 75 DEG C; CONNECTION: THD; BODY MATERIAL: STL CAST; TRIM: BONNET CS; FACE TO FACE LENGTH: 150.5 X 90 MM; OPERATED: PILOT; MODEL NO: BT-03-32","REXROTH, SIZANANI VALVES","RELIEF","3 IN","STL CAST","25 MPA","BONNET CS","THD","150.5 X 90 MM","N/A","PILOT","VARIOUS","-15 TO 75 DEG C","BT-03-32"]
["Ingula Pumped Storage Scheme",783932,"VALVE, BUTTERFLY: TYPE: VALVE BUTTERFLY; VALVE SIZE: DN 80 MM; DESIGN RATING: PN16 BAR; TEMPERATURE RATING: 95; CONNECTION: RUBBER SEALING; BODY MATERIAL: GG-25; FACE TO FACE LENGTH: 46 MM; OPERATED: ACTUATOR","SUPERPUMP, KLINGER MZANSI","BUTTERFLY; VALVE BUTTERFLY","DN 80 MM","GG-25","PN16 BAR","STAINLESSTEEL","RUBBER SEALING","46 MM","N/A","ACTUATOR","WATER",95]
["Gourikwa OCGT Power Station",233792,"VALVE, SOLENOID: PIPE SIZE: DN15; STYLE: 2 WAY; POTENTIAL: 220 VDC; DESIGN RATING: 100 BAR; CONNECTION: FLANGE; BODY MATERIAL: GR 1.4404/1.4571; OPERATED: NO; ENCLOSURE RATING: IP65; MEDIUM: HEIZOL; CURRENT: 0.22 A; ORIFICE SIZE: DN 15; COIL: 220 V DC; MANUF P/N: FK15NO1E; SUPPL P/N: A2A50187268; REFERENCE NO: PB0000144283; 503443; 2.5 M3/HR; WITH 4 X 14 MM DIA HOLES DRILLED INTO FLANGE","Muller Coax","SOLENOID","DN15; DN 15","GR 1.4404/1.4571","100 BAR",null,"FLANGE",null,null,"NO","HEIZOL",null,"FK15NO1E; A2A50187268; PB0000144283","220 VDC; 0.22 A; 220 V DC; IP65"]
["Gourikwa OCGT Power Station",233844,"VALVE, CHECK: BODY MATERIAL: CI; SUPPL P/N: MBV30AA201; C5V08311B5; LIFTING OIL; KKS; FOR USE ON LIFTING OIL PUMP MBV BASE PIPING ON GT AUX SYSTEM","Parker","CHECK",null,"CI",{"$nulls":6},"LIFTING OIL PUMP MBV BASE PIPING ON GT AUX SYSTEM",null,"MBV30AA201"]
["Gourikwa OCGT Power Station",233849,"VALVE, BALL: VALVE SIZE: 1 IN; DESIGN RATING: 40 BAR; CONNECTION: BSP; BODY MATERIAL: STAINLESS STEEL; OPERATED: LEVER; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: PTFE; SUPPL P/N: MBV23AA412; REFERENCE NO: SLV3800141; MBV25AA401; WITH ATTACHMENT, KKS; FOR USE ON LUBE OIL FILTER ON MBV BASE PIPING ON GT AUX SYSTEM",null,"BALL","1 IN","STAINLESS STEEL","40 BAR","STAINLESS STEEL","BSP",null,null,"LEVER","LUBE OIL FILTER ON MBV BASE PIPING ON GT AUX SYSTEM",null,"MBV23AA412; SLV3800141",null,"PTFE"]
["Gourikwa OCGT Power Station",233850,"VALVE: TYPE: ISOLATING; VALVE SIZE: NB 4; DESIGN RATING: 400 BAR; CONNECTION: BSP; OPERATED: HANDWHEEL; BODY MATERIAL: 1.046; STYLE: ISOLATE/VENT; REFERENCE NO: MBV31AA301; MBV31AA305; MBV21AA301; MBV23AA301; FOR USE ON GT AUX SYSTEMS",null,"ISOLATING","NB 4",1.046,"400 BAR",null,"BSP",null,null,"HANDWHEEL","GT AUX SYSTEMS",null,"MBV31AA301"]
["Gourikwa OCGT Power Station",233851,"VALVE: TYPE: BALANCE; VALVE SIZE: 3/8 IN; DESIGN RATING: 16 BAR; TEMPERATURE RATING: 80-100 DEG C; CONNECTION: 3/8 IN-BSPP; OPERATED: KNOB; BODY MATERIAL: STL HARDENED BS 970; SPECIFICATION: 305000; SPECIAL FEATURES: HAND WHEEL; STL VERSION; MANUF P/N: 305000; REFERENCE NO: SLV3800141; MBV25AA252; FOR USE ON LUBE OIL FILTER ON MBV BASE PIPING ON GT AUX SYSTEM",null,"BALANCE","3/8 IN","STL HARDENED BS 970","16 BAR",null,"3/8 IN-BSPP",null,null,"KNOB","LUBE OIL FILTER ON MBV BASE PIPING ON GT AUX SYSTEM","80-100 DEG C","305000; SLV3800141"]
["Gourikwa OCGT Power Station",233857,"VALVE, BUTTERFLY: TYPE: WAFER; VALVE SIZE: 150 MM; DESIGN RATING: PN16; TEMPERATURE RATING: -10 TO 80 DEG C; CONNECTION: FLANGE; BODY MATERIAL: STEEL; OPERATED: HANDLEVER; TRIM: STAINLESS STEEL; SOFTGOODS: RUBBER; REFERENCE NO: MBV21AA254; ECLS 71391; FOR USE ON MBV BASE PIPING ON GT AUX SYSTEM",null,"BUTTERFLY; WAFER","150 MM","STEEL","PN16","STAINLESS STEEL","FLANGE",null,null,"HANDLEVER","MBV BASE PIPING ON GT AUX SYSTEM","-10 TO 80 DEG C","MBV21AA254",null,"RUBBER"]
["Gourikwa OCGT Power Station",233871,"VALVE, RELIEF: BODY MATERIAL: CAST IRON; DESIGN RATING: 210 BAR; SUPPL P/N: MBA30AA191; R5V 08 593 32 A5 152 210; REFERENCE NO: SLV 3720522; PARKER; KKS: FOR LIFTING OIL PUMP ON GT AUX SYSTEM","Parker","RELIEF",null,"CAST IRON","210 BAR",{"$nulls":7},"MBA30AA191; SLV 3720522"]
["Gourikwa OCGT Power Station",233872,"VALVE, RELIEF: BODY MATERIAL: CI; SUPPL P/N: R4V06 535 30 A5; MBV31AA151; REFERENCE NO: SLV3860114; PARKER, KKS; FOR CONTROL BLOCK LIFTING OIL ON MBV BASE PIPING ON GT AUX SYSTEM","Parker","RELIEF",null,"CI",{"$nulls":8},"R4V06 535 30 A5; SLV3860114"]
["Gourikwa OCGT Power Station",233891,"VALVE, BALL: VALVE SIZE: 1/4 IN; DESIGN RATING: 65; CONNECTION: THD; BODY MATERIAL: STAINLESS STEEL; OPERATED: LEVER; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: TEFLON; SUPPL P/N: MBV50AA503; KKS; USED ON MBV BASE PIPING ON GT AUX SYSTEMS",null,"BALL","1/4 IN","STAINLESS STEEL",65,"STAINLESS STEEL","THD",null,null,"LEVER","MBV BASE PIPING ON GT AUX SYSTEMS",null,"MBV50AA503",null,"TEFLON"]
["Gourikwa OCGT Power Station",233892,"VALVE, BALL: VALVE SIZE: 1/2 IN; DESIGN RATING: 65 BAR; CONNECTION: THD; BODY MATERIAL: STAINLESS STEEL; OPERATED: LEVER; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: TEFLON; SUPPL P/N: MBV21AA403; KKS; USED ON MBV BASE PIPING ON GT AUX SYSTEMS",null,"BALL","1/2 IN","STAINLESS STEEL","65 BAR","STAINLESS STEEL","THD",null,null,"LEVER","MBV BASE PIPING ON GT AUX SYSTEMS",null,"MBV21AA403",null,"TEFLON"]
["Gourikwa OCGT Power Station",233893,"VALVE, BALL: VALVE SIZE: 3/4 IN; DESIGN RATING: 40; CONNECTION: THD; BODY MATERIAL: STAINLESS STEEL; OPERATED: LEVER; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: TEFLON; SUPPL P/N: MBV26AA401; KKS; USED ON MBV BASE PIPING ON GT AUX SYSTEMS",null,"BALL","3/4 IN","STAINLESS STEEL",40,"STAINLESS STEEL","THD",null,null,"LEVER","MBV BASE PIPING ON GT AUX SYSTEMS",null,"MBV26AA401",null,"TEFLON"]
["Gourikwa OCGT Power Station",233895,"VALVE, RELIEF: VALVE SIZE: 3/4 X 1/2 IN; SET PRESSURE: 10 BAR; CONNECTION: BSP; BODY MATERIAL: BRASS; TRIM: BRASS; OPERATED: PRESSURE; SUPPL P/N: MBV23AA191; KKS; USED ON GT AUX SYSTEMS",null,"RELIEF","3/4 X 1/2 IN","BRASS","10 BAR","BRASS","BSP",null,null,"PRESSURE","GT AUX SYSTEMS",null,"MBV23AA191"]
["Gourikwa OCGT Power Station",233896,"VALVE: TYPE: THROTTLE; OPERATED: KEY LOCK; BODY MATERIAL: STL; REFERENCE NO: MBV31AA285; USED ON CONTROL BLOCK ON MBV BASE PIPING ON GT AUX SYSTEMS",null,"THROTTLE",null,"STL",{"$nulls":5},"KEY LOCK","CONTROL BLOCK ON MBV BASE PIPING ON GT AUX SYSTEMS",null,"MBV31AA285"]
["Gourikwa OCGT Power Station",233898,"VALVE, BALL: VALVE SIZE: 2 IN; DESIGN RATING: 40 BAR; CONNECTION: THD; BODY MATERIAL: STAINLESS STEEL; OPERATED: LEVER; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: TEFLON; SUPPL P/N: MBV10AA401; KKS; USED ON MBV BASE PIPING ON GT AUX SYSTEMS",null,"BALL","2 IN","STAINLESS STEEL","40 BAR","STAINLESS STEEL","THD",null,null,"LEVER","MBV BASE PIPING ON GT AUX SYSTEMS",null,"MBV10AA401",null,"TEFLON"]
["Gourikwa OCGT Power Station",233901,"VALVE, CHECK: TYPE: NON RETURN; VALVE SIZE: 150 MM; DESIGN RATING: 10-40 BAR; CONNECTION: FLANGE; STYLE: 1 WAY; TRIM: 1.4408; GRADE: 1.057; SUPPL P/N: MBV21AA201; KKS, USED ON MBV BASE PIPING ON GT AUX SYSTEMS",null,"CHECK; NON RETURN","150 MM",null,"10-40 BAR",1.4408,"FLANGE",{"$nulls":3},"MBV BASE PIPING ON GT AUX SYSTEMS",null,"MBV21AA201"]
["Gourikwa OCGT Power Station",235772,"VALVE: TYPE: ISOLATING GAUGE; VALVE SIZE: NB 4; DESIGN RATING: PN400; CONNECTION: THD 1/2 IN; OPERATED: MANUAL; BODY MATERIAL: 1.4571; STYLE: 1 WAY; TRIM: GR 1.4571; SOFTGOODS: GR 1.4571; WITH ONE KNOB; USED ON GAS 1 AUX SYSTEM",null,"ISOLATING GAUGE","NB 4",1.4571,"PN400","GR 1.4571","THD 1/2 IN",null,null,"MANUAL","GAS 1 AUX SYSTEM",{"$nulls":3},"GR 1.4571"]
["Gourikwa OCGT Power Station",235781,"VALVE, CHECK: VALVE SIZE: 80; DESIGN RATING: PN16; BODY MATERIAL: BRZ; OPERATED: SPRING; STYLE: 1 WAY; TRIM: DISC SS; SOFTGOODS: STAINLESS STEEL; SUPPL P/N: RK71; NON RETURN; WITH SPIRAL CENTERING RING; USED ON GAS 1 AUX SYSTEM; TEMPERATURE RATING: 13 BAR AT 250 DEG CEL",null,"CHECK",80,"BRZ","PN16","DISC SS",{"$nulls":3},"SPRING","GAS 1 AUX SYSTEM","13 BAR AT 250 DEG CEL","RK71",null,"STAINLESS STEEL"]
["Gourikwa OCGT Power Station",235783,"VALVE, RELIEF: VALVE SIZE: 3/4 IN; TEMPERATURE RATING: 130 DEG C; CONNECTION: FEMALE THD; BODY MATERIAL: CRNIMO-STAHL; OPERATED: AIR; DESIGN RATING: PN16; PRESSURE RANGE: 0-16 BAR; REFERENCE NO: 7146002; MANKENBURG; USED ON GAS 1 AUX SYSTEM.","Mankenburg","RELIEF","3/4 IN","CRNIMO-STAHL","PN16; 0-16 BAR",null,"FEMALE THD",null,null,"AIR","GAS 1 AUX SYSTEM","130 DEG C",7146002]
["Gourikwa OCGT Power Station",238889,"VALVE: TYPE: GAGE ISOLATING; VALVE SIZE: 4 MM; DESIGN RATING: PN400; CONNECTION: 1/2 IN-BSP; OPERATED: MANUAL; BODY MATERIAL: CI; STYLE: 1 WAY; TRIM: CI; REFERENCE NO: 061462-9515.002; COMPLETE WITH BLEED DOWN SCREW; USED ON GAS 1 PLANT","Wika","GAGE ISOLATING","4 MM","CI","PN400","CI","1/2 IN-BSP",null,null,"MANUAL","GAS 1 PLANT",null,"061462-9515.002"]
["Gourikwa OCGT Power Station",239052,"VALVE, BALL: VALVE SIZE: 1/2 IN; DESIGN RATING: 16 BAR; CONNECTION: THD FEMALE; BODY MATERIAL: STAINLESS STEEL; OPERATED: WING GREEN; STYLE: 1 WAY; TRIM: TEFLON; FOR USE ON GAS 1 PLANT",null,"BALL","1/2 IN","STAINLESS STEEL","16 BAR","TEFLON","THD FEMALE",null,null,"WING GREEN","GAS 1 PLANT"]
["Gourikwa OCGT Power Station",239053,"VALVE, RELIEF: VALVE SIZE: 1 IN; SET PRESSURE: 5.6 BAR; CONNECTION: THD; BODY MATERIAL: CI; OPERATED: PRESSURE; STYLE: 1 WAY; SUPPL P/N: 4593.2504; FOR USE ON GAS 1 PLANT",null,"RELIEF","1 IN","CI","5.6 BAR",null,"THD",null,null,"PRESSURE","GAS 1 PLANT",null,4593.2504]
["Gourikwa OCGT Power Station",239054,"VALVE, RELIEF: VALVE SIZE: 1 IN; SET PRESSURE: 6 BAR; CONNECTION: THD; BODY MATERIAL: CI; OPERATED: PRESSURE; STYLE: 1 WAY; SUPPL P/N: 4603.7863; TYPE SAFETY; TYPE LESER; FOR USE ON GAS 1 PLANT","SAFETY; LESER","RELIEF","1 IN","CI","6 BAR",null,"THD",null,null,"PRESSURE","GAS 1 PLANT",null,4603.7863]
["Gourikwa OCGT Power Station",239649,"VALVE, BALL: VALVE SIZE: 1/2 IN; DESIGN RATING: 16; TEMPERATURE RATING: -20 TO 130 DEG C; CONNECTION: THD 1/2 IN; BODY MATERIAL: BRS NICKEL PLTD; FACE TO FACE LENGTH: 50 MM; OPERATED: LEVER; STYLE: 1 WAY VALVE AND PLUG; APPLICATION: WATER; SUPPL P/N: 305220108",null,"BALL","1/2 IN","BRS NICKEL PLTD",16,null,"THD 1/2 IN","50 MM",null,"LEVER","WATER","-20 TO 130 DEG C",305220108]
["Gourikwa OCGT Power Station",239669,"VALVE, SOLENOID: PIPE SIZE: DN15; STYLE: 2/2 WAY; POTENTIAL: 24 VDC; DESIGN RATING: 0-40 BAR; CONNECTION: FLANGE; BODY MATERIAL: STAINLESS STEEL; OPERATED: SOLENOID; ENCLOSURE RATING: IP65; MEDIUM: DEMINIRALIZED WATER 70; POWER: 24 V X 1.6 A; CURRENT: 1.6 A; ORIFICE SIZE: DN 15; SOFTGOODS: SEAL VITON; APPLICATION: DEMIN WATER; SPECIFICATION: COAX VALVE; MANUF P/N: FK15NC; REFERENCE NO: 513465","Coax","SOLENOID","DN15; DN 15","STAINLESS STEEL","0-40 BAR",null,"FLANGE",null,null,"SOLENOID","DEMINIRALIZED WATER 70; DEMIN WATER",null,"FK15NC; 513465","24 VDC; 24 V X 1.6 A; 1.6 A; IP65","SEAL VITON"]
["Gourikwa OCGT Power Station",239684,"VALVE, RELIEF: VALVE SIZE: 1 IN; SET PRESSURE: 10 BAR; CONNECTION: THD; BODY MATERIAL: BRASS; TRIM: BRASS; OPERATED: PRESSURE; DESIGN RATING: 25 BAR; PRESSURE RANGE: 0-25 BAR; SUPPL P/N: TUVSV 03-581 18",null,"RELIEF","1 IN","BRASS","25 BAR; 0-25 BAR; 10 BAR","BRASS","THD",null,null,"PRESSURE",null,null,"TUVSV 03-581 18"]
["Gourikwa OCGT Power Station",239791,"VALVE, RELIEF: VALVE SIZE: DN 32, 140 MM; SET PRESSURE: 22 BAR; CONNECTION: FLANGE, 140 MM; BODY MATERIAL: STAINLESS STEEL; TRIM: STAINLESS STEEL; FACE TO FACE LENGTH: 275 MM; OPERATED: SPRING; APPLICATION: TURBINE PURGE WATER OVERFLOW CONTROL; GRADE: 1.4408; DESIGN RATING: PN40; VALVE MADE OF CAST STEEL; SEAT,CONE,GUID CONE SPINDLE OF HIGH QUALITY STEEL; CENTRAL SPRING, DIN PN40; WILLEM SCHLEY HAMBURG - OVERFLOW VALVE MODEL T27","WILLEM SCHLEY HAMBURG - OVERFLOW VALVE; Willem Schley","RELIEF","DN 32, 140 MM","STAINLESS STEEL","PN40; 22 BAR","STAINLESS STEEL","FLANGE, 140 MM","275 MM",null,"SPRING","TURBINE PURGE WATER OVERFLOW CONTROL",{"$nulls":3},"L"]
["Gourikwa OCGT Power Station",239795,"VALVE, CHECK: TYPE: NON RETURN; VALVE SIZE: 150 MM; DESIGN RATING: PN40; CONNECTION: FLANGE; BODY MATERIAL: STAINLESS STEEL; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SUPPL P/N: RK86A","Gestra","CHECK; NON RETURN","150 MM","STAINLESS STEEL","PN40","STAINLESS STEEL","FLANGE",{"$nulls":5},"RK86A"]
["Gourikwa OCGT Power Station",250048,"VALVE, CHECK: APPLICATION: CENTRIFUGES; MANUF P/N: 176289482; CAPACITY 2.8 L/MIN","Alva-Laval","CHECK",{"$nulls":8},"CENTRIFUGES",null,176289482]
["Gourikwa OCGT Power Station",250049,"VALVE, CHECK: APPLICATION: CENTRIFUGES; MANUF P/N: 176289486; OPERATED FLOW, CAPACITY 23 L/MIN","Alva-Laval","CHECK",{"$nulls":8},"CENTRIFUGES",null,176289486]
["Gourikwa OCGT Power Station",250052,"VALVE, SOLENOID: PIPE SIZE: 3/4 X 1 IN; STYLE: 4/2 WAY; POTENTIAL: 24 VDC; DESIGN RATING: 17 BAR; CONNECTION: NPT; BODY MATERIAL: BRASS; OPERATED: ELECTRONIC; ENCLOSURE RATING: IP65; MEDIUM: OIL/WATER; POWER: 11.6 W; CURRENT: 0.48 A; ORIFICE SIZE: 19 MM; COIL: SINGLE; APPLICATION: SSS CLUTCH; SPECIFICATION: SOLINOID VALVE; MANUF P/N: SC8344G076; REFERENCE NO: SC8344G076",null,"SOLENOID","3/4 X 1 IN; 19 MM","BRASS","17 BAR",null,"NPT",null,null,"ELECTRONIC","OIL/WATER; SSS CLUTCH",null,"SC8344G076","24 VDC; 11.6 W; 0.48 A; SINGLE; IP65"]
["Gourikwa OCGT Power Station",250052,"VALVE, SOLENOID: PIPE SIZE: 3/4 X 1 IN; STYLE: 4/2 WAY; POTENTIAL: 24 VDC; DESIGN RATING: 17 BAR; CONNECTION: NPT; BODY MATERIAL: BRASS; OPERATED: ELECTRONIC; ENCLOSURE RATING: IP65; MEDIUM: OIL/WATER; POWER: 11.6 W; CURRENT: 0.48 A; ORIFICE SIZE: 19 MM; COIL: SINGLE; APPLICATION: SSS CLUTCH; SPECIFICATION: SOLINOID VALVE; MANUF P/N: SC8344G076; REFERENCE NO: SC8344G076",null,"SOLENOID","3/4 X 1 IN; 19 MM","BRASS","17 BAR",null,"NPT",null,null,"ELECTRONIC","OIL/WATER; SSS CLUTCH",null,"SC8344G076","24 VDC; 11.6 W; 0.48 A; SINGLE; IP65"]
["Gourikwa OCGT Power Station",257026,"VALVE, BALL: VALVE SIZE: 40 MM; DESIGN RATING: 100; TEMPERATURE RATING: -10 TO 200 DEG C; CONNECTION: FLANGE; BODY MATERIAL: STEEL; FACE TO FACE LENGTH: 250; OPERATED: ACTUATOR ELECTRIC; GRADE: I54; TYPE: PREMIX","Argus","BALL; PREMIX","40 MM","STEEL",100,null,"FLANGE",250,null,"ACTUATOR ELECTRIC",null,"-10 TO 200 DEG C"]
["Gourikwa OCGT Power Station",553121,"VALVE, SOLENOID: PIPE SIZE: 1/2 IN; STYLE: (2) PIPE CONNECTIONS; (1) SOLENOID; POTENTIAL: 220 VDC; DESIGN RATING: 0-100 BAR; CONNECTION: TERMINAL; BODY MATERIAL: GS/BRS; OPERATED: COIL; ENCLOSURE RATING: IP65; MEDIUM: DIESEL; POWER: 40 W; CURRENT: 0.17 A DC; ORIFICE SIZE: G 1/2 IN; COIL: 220 VOLT DC INSULATION CLASS - H; SOFTGOODS: VITON SEALS; APPLICATION: DIFFUSION/PREMIX FUEL LINES V9214 GAS TURBINES; SPECIFICATION: MK15NC2E; CLASSIFICATION: E X NA11 T3; MANUF P/N: MK15NC2E; 523181; TERMINAL 130 X M15 X 1.5 MM","Muller Coax","SOLENOID","1/2 IN; G 1/2 IN","GS/BRS","0-100 BAR",null,"TERMINAL",null,null,"COIL","DIESEL; DIFFUSION/PREMIX FUEL LINES V9214 GAS TURBINES",null,"MK15NC2E","220 VDC; 40 W; 0.17 A DC; 220 VOLT DC INSULATION CLASS - H; IP65; E X NA11 T3","VITON SEALS"]
["Gourikwa OCGT Power Station",553122,"VALVE: TYPE: SOLENOID COAXIAL; VALVE SIZE: G10/0; DESIGN RATING: 40 BAR; TEMPERATURE RATING: -40 TO 100 DEG C; CONNECTION: 1/2 IN; OPERATED: ELECTRIC COIL 220VAC; BODY MATERIAL: BRASS; SPECIFICATION: VALVE; SOFTGOODS: VITON; SPECIAL FEATURES: VITON SEAL; MANUF P/N: MK25DRN01E; 510038","Coax","SOLENOID COAXIAL","G10/0","BRASS","40 BAR",null,"1/2 IN",null,null,"ELECTRIC COIL 220VAC",null,"-40 TO 100 DEG C","MK25DRN01E",null,"VITON"]
["Gourikwa OCGT Power Station",553123,"VALVE: TYPE: SOLONOID COAXIAL; VALVE SIZE: PN40; DESIGN RATING: 0-40 BAR; TEMPERATURE RATING: -40 TO 100 DEG C; CONNECTION: FLANGE PN40; OPERATED: ELECTRIC COIL 230VAC; BODY MATERIAL: BRASS; SPECIFICATION: VALVE; SOFTGOODS: VITON; SPECIAL FEATURES: VITON SEALS; MANUF P/N: 515259; FK25NC1E","Coax","SOLONOID COAXIAL","PN40","BRASS","0-40 BAR",null,"FLANGE PN40",null,null,"ELECTRIC COIL 230VAC",null,"-40 TO 100 DEG C",515259,null,"VITON"]
["Gourikwa OCGT Power Station",553124,"VALVE: TYPE: SOLONOID COAXIAL; VALVE SIZE: PN40; DESIGN RATING: 0-40 BAR; TEMPERATURE RATING: -40 TO 100 DEG C; CONNECTION: FLANGE; OPERATED: ELECTRIC COIL 240VAC; BODY MATERIAL: BRASS; SPECIFICATION: VALVE; SOFTGOODS: VITON; SPECIAL FEATURES: VITON SEALS; MANUF P/N: 527506; FK25NC","Coax","SOLONOID COAXIAL","PN40","BRASS","0-40 BAR",null,"FLANGE",null,null,"ELECTRIC COIL 240VAC",null,"-40 TO 100 DEG C",527506,null,"VITON"]
["Gourikwa OCGT Power Station",553125,"VALVE: TYPE: SOLONOID COAXIAL; VALVE SIZE: NB8 MM; DESIGN RATING: 0-150 BAR; TEMPERATURE RATING: 55 DEG C; CONNECTION: 3/8 IN THREAD; OPERATED: ELECTRIC COIL 220VDC; BODY MATERIAL: BRASS; SPECIFICATION: VALVE; SOFTGOODS: VITON; MANUF P/N: 503507; ECD-H10NO2E","Coax","SOLONOID COAXIAL","NB8 MM","BRASS","0-150 BAR",null,"3/8 IN THREAD",null,null,"ELECTRIC COIL 220VDC",null,"55 DEG C",503507,null,"VITON"]
["Gourikwa OCGT Power Station",553126,"VALVE: TYPE: COAXIAL SOLENOID; VALVE SIZE: G11/4; 38 MM; DESIGN RATING: 0-100 BAR; TEMPERATURE RATING: -40 TO 100 DEG C; CONNECTION: 1-1/4 IN THREAD; OPERATED: ELECTRIC COIL 220VDC; BODY MATERIAL: BRASS; SOFTGOODS: VITON; MANUF P/N: 500479; MK25NC1E","Coax","COAXIAL SOLENOID","G11/4","BRASS","0-100 BAR",null,"1-1/4 IN THREAD",null,null,"ELECTRIC COIL 220VDC",null,"-40 TO 100 DEG C",500479,null,"VITON"]
["Gourikwa OCGT Power Station",553127,"VALVE: TYPE: SOLENOID COAXIAL; VALVE SIZE: PN100; DESIGN RATING: 0-100 BAR; TEMPERATURE RATING: -40 TO 100 DEG C; FACE TO FACE LENGTH: 241 MM; CONNECTION: THREAD/FLANGE; OPERATED: ELECTRIC COIL 220VDC; BODY MATERIAL: BRASS; SPECIFICATION: VALVE; SOFTGOODS: VITON; SPECIAL FEATURES: VITON SEALS; MANUF P/N: 527372; FKI5NC1E","Coax","SOLENOID COAXIAL","PN100","BRASS","0-100 BAR",null,"THREAD/FLANGE","241 MM",null,"ELECTRIC COIL 220VDC",null,"-40 TO 100 DEG C",527372,null,"VITON"]
["Gourikwa OCGT Power Station",553128,"VALVE: TYPE: SOLONOID COAXIAL; VALVE SIZE: G1/2; DESIGN RATING: 0-100 BAR; TEMPERATURE RATING: -40 TO 100 DEG C; CONNECTION: THREAD/FLANGE; OPERATED: ELECTRIC COIL 230VAC; BODY MATERIAL: BRASS; SPECIFICATION: VALVE; SOFTGOODS: VITON; MANUF P/N: MK15NC1E; 520496","Coax","SOLONOID COAXIAL","G1/2","BRASS","0-100 BAR",null,"THREAD/FLANGE",null,null,"ELECTRIC COIL 230VAC",null,"-40 TO 100 DEG C","MK15NC1E",null,"VITON"]
["Gourikwa OCGT Power Station",553129,"VALVE: TYPE: INLINE SOLENOID; VALVE SIZE: G1/2 IN-BSPP; DESIGN RATING: 0-40 BAR; TEMPERATURE RATING: -40 TO 100 DEG C; FACE TO FACE LENGTH: 184 MM; CONNECTION: THD; OPERATED: ELECTRIC COIL 220VDC; BODY MATERIAL: GS/BRS; STYLE: 2/2 WAY DIRECT ACTING; TRIM: BODY MATERIAL BRASS/GALVANISED STEEL; SPECIFICATION: VALVE; SOFTGOODS: VITON; SPECIAL FEATURES: 2 X INDUCTIVE PROXIMITY SWITCHES/SAME DIRECTION SWITCHING; MANUF P/N: 503506; MK15NC2E","Muller Coax","INLINE SOLENOID","G1/2 IN-BSPP","GS/BRS","0-40 BAR","BODY MATERIAL BRASS/GALVANISED STEEL","THD","184 MM",null,"ELECTRIC COIL 220VDC",null,"-40 TO 100 DEG C",503506,null,"VITON"]
["Gourikwa OCGT Power Station",585702,"VALVE, SOLENOID: PIPE SIZE: G3/8 IN; STYLE: 2/2 WAY; POTENTIAL: 220 VDC; DESIGN RATING: 0-150 BAR; CONNECTION: THD; BODY MATERIAL: BRASS; OPERATED: SOLENOID; ENCLOSURE RATING: IP65; MEDIUM: FUEL/OIL; ORIFICE SIZE: 10 MM; SOFTGOODS: VITON SEALS; APPLICATION: FUEL/OIL; SPECIFICATION: 516348; CLASSIFICATION: ZONE 2; MANUF P/N: ECD-H10NO2E; 2 LIMIT SWITCHES, 55 DEG; HIGH PRESSURE","Muller Coax","SOLENOID","G3/8 IN; 10 MM","BRASS","0-150 BAR",null,"THD",null,null,"SOLENOID","FUEL/OIL",null,"ECD-H10NO2E","220 VDC; IP65; ZONE 2","VITON SEALS"]
["Gourikwa OCGT Power Station",588761,"VALVE, BUTTERFLY: TYPE: SWIVEL; VALVE SIZE: 400 MM; DESIGN RATING: 6 BAR; TEMPERATURE RATING: 270 DEG C; CONNECTION: FLANGE; BODY MATERIAL: STEEL WELDMENT; FACE TO FACE LENGTH: 310 MM; OPERATED: ACTUATOR PNEUMATIC; TRIM: FLEXIBLE PRESS FORMED; SOFTGOODS: PTFE COMPOUND; APPLICATION: TURBINE COMPRESSOR; GRADE: PN10; DIN 2632; DRAWING NO: 1.5055B REV 0; INCLUDING ACTUATOR: ACTUATOR POSITION SLV 3540043 (TOP)","Friedrich Krombach","BUTTERFLY; SWIVEL","400 MM","STEEL WELDMENT","6 BAR","FLEXIBLE PRESS FORMED","FLANGE","310 MM",null,"ACTUATOR PNEUMATIC; ACTUATOR POSITION SLV 3540043 (TOP)","TURBINE COMPRESSOR","270 DEG C","1.5055B REV 0",null,"PTFE COMPOUND"]
["Gourikwa OCGT Power Station",593549,"VALVE, BUTTERFLY: TYPE: SWIVEL; VALVE SIZE: 400 MM; DESIGN RATING: 6 BAR; TEMPERATURE RATING: 270 DEG C; CONNECTION: FLANGE; BODY MATERIAL: STEEL WELDMENT; FACE TO FACE LENGTH: 310 MM; OPERATED: ACTUATOR PNEUMATIC; TRIM: FLEXIBLE PRESS FORMED; SOFTGOODS: PTFE COMPOUND; APPLICATION: TURBINE COMPRESSOR; GRADE: PN10; DIN 2632; DRAWING NO: 1.5055B REV 0; INCLUDING ACTUATOR; ACTUATOR POSITION SLV 3540041 L/H","Friedrich Krombach","BUTTERFLY; SWIVEL","400 MM","STEEL WELDMENT","6 BAR","FLEXIBLE PRESS FORMED","FLANGE","310 MM",null,"ACTUATOR PNEUMATIC","TURBINE COMPRESSOR","270 DEG C","1.5055B REV 0",null,"PTFE COMPOUND"]
["Gourikwa OCGT Power Station",593550,"VALVE, BUTTERFLY: TYPE: SWIVEL; VALVE SIZE: 400 MM; DESIGN RATING: 6 BAR; TEMPERATURE RATING: 270 DEG C; CONNECTION: FLANGE; BODY MATERIAL: STEEL WELDMENT; FACE TO FACE LENGTH: 310 MM; OPERATED: ACTUATOR PNEUMATIC; TRIM: FLEXIBLE PRESS FORMED; SOFTGOODS: PTFE COMPOUND; APPLICATION: TURBINE COMPRESSOR; GRADE: PN10; DIN 2632; DRAWING NO: 1.5055B REV 0; INCLUDING ACTUATOR; ACTUATOR POSITION SLV 3540042 R/H","Friedrich Krombach","BUTTERFLY; SWIVEL","400 MM","STEEL WELDMENT","6 BAR","FLEXIBLE PRESS FORMED","FLANGE","310 MM",null,"ACTUATOR PNEUMATIC","TURBINE COMPRESSOR","270 DEG C","1.5055B REV 0",null,"PTFE COMPOUND"]
["Gourikwa OCGT Power Station",593794,"KIT: TYPE: SEAL; APPLICATION: CHANGE OVER VALVE HDD 91; COMPRISING: O-RINGS; SUPPORT RINGS; MANUF P/N: 318517; ALL O RINGS FROM VITON MATERIAL - HDD91 CHANGE OVER VALVE",null,"SEAL",{"$nulls":8},"CHANGE OVER VALVE HDD 91",null,318517]
["Gourikwa OCGT Power Station",593797,"KIT: TYPE: SEAL; APPLICATION: CHANGE OVER VALVE HDD 170; COMPRISING: O-RINGS; SUPPORT RINGS; MANUF P/N: 308333; ALL O RINGS FROM VITON MATERIAL - HDD 170 CHANGE OVER VALVE",null,"SEAL",{"$nulls":8},"CHANGE OVER VALVE HDD 170",null,308333]
["Gourikwa OCGT Power Station",607158,"VALVE, BALL: VALVE SIZE: 40 MM; DESIGN RATING: 100 BAR; TEMPERATURE RATING: -10 TO 200 DEG C; CONNECTION: FLANGE; BODY MATERIAL: STEEL; FACE TO FACE LENGTH: 850 MM; OPERATED: ACTUATOR/ELECTRICAL; GRADE: I54; TYPE: FUEL DIFFUSION; MANUF P/N: 5100046637-100; 6211-0100-670289/G84/G82G; VALVE AND ACTUATOR ASSEMBLY","Argus","BALL; FUEL DIFFUSION","40 MM","STEEL","100 BAR",null,"FLANGE","850 MM",null,"ACTUATOR/ELECTRICAL",null,"-10 TO 200 DEG C","5100046637-100"]
["Gourikwa OCGT Power Station",612657,"VALVE, BALL: VALVE SIZE: DN 40; DESIGN RATING: PN100; TEMPERATURE RATING: -10 TO 200 DEG C; CONNECTION: FLANGE; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 300 MM; OPERATED: ELECTRICAL MOTOR; STYLE: 3 WAY; TYPE: PREMIX; SUPPL P/N: 6211-0100-670852MOD/-G85GH...M; VALVE AND ACTUATOR ASSEMBLY; ARGUS E25 ELECTRIC ACTUATOR, VALVE AND ELECTRIC ACTUATOR ASSEMBLY A2A50296201/ PB0000279980","Argus","BALL; PREMIX","DN 40","STAINLESS STEEL","PN100",null,"FLANGE","300 MM",null,"ELECTRICAL MOTOR",null,"-10 TO 200 DEG C","6211-0100-670852MOD/-G85GH...M"]
["Gourikwa OCGT Power Station",613732,"VALVE: TYPE: SOL; VALVE SIZE: 15 MM; TEMPERATURE RATING: MAX 160 DEG C; FACE TO FACE LENGTH: 130 MM; CONNECTION: FLANGE; OPERATED: ELECTRICAL; BODY MATERIAL: STAINLESS STEEL; OEM P/N: 12-EVF 5R U.XN.P.09.29; A2A50268346; SUPPL P/N: 799.010.010.0421; 220 VDC","Argus","SOL","15 MM","STAINLESS STEEL",null,null,"FLANGE","130 MM",null,"ELECTRICAL",null,"MAX 160 DEG C","12-EVF 5R U.XN.P.09.29; 799.010.010.0421"]
["Gourikwa OCGT Power Station",613733,"VALVE: TYPE: SOL; VALVE SIZE: 15 MM; TEMPERATURE RATING: MAX 160 DEG C; FACE TO FACE LENGTH: 130 MM; CONNECTION: FLANGE; OPERATED: ELECTRICAL; BODY MATERIAL: STAINLESS STEEL; OEM P/N: 12-EVDF 3R XN.W.U.P.09.29; SUPPL P/N: 799.010.010.0422; A2A50268347; 220 VDC","Uni Gerate","SOL","15 MM","STAINLESS STEEL",null,null,"FLANGE","130 MM",null,"ELECTRICAL",null,"MAX 160 DEG C","12-EVDF 3R XN.W.U.P.09.29; 799.010.010.0422"]
["Gourikwa OCGT Power Station",613741,"VALVE: TYPE: NON RETURN,WAFER; VALVE SIZE: 54 MM; DESIGN RATING: 160 BAR; TEMPERATURE RATING: 300 DEG C; FACE TO FACE LENGTH: 25 MM; CONNECTION: COUPLING; OPERATED: PNEUMATIC; BODY MATERIAL: STAINLESS STEEL; STYLE: WAFER; TRIM: DISC SS; OEM P/N: A2A50005975; SUPPL P/N: 700.050.010.1028",null,"NON RETURN,WAFER","54 MM","STAINLESS STEEL","160 BAR","DISC SS","COUPLING","25 MM",null,"PNEUMATIC",null,"300 DEG C","A2A50005975; 700.050.010.1028"]
["Gourikwa OCGT Power Station",621637,"SET: TYPE: STOP VALVE; OEM P/N: A2A50314606; SUPPL P/N: PG0031759200",null,"STOP VALVE",{"$nulls":10},"A2A50314606; PG0031759200"]
["Gourikwa OCGT Power Station",622490,"VALVE, SOLENOID: PIPE SIZE: DN25; STYLE: 1/2; POTENTIAL: 220 V; DESIGN RATING: PN40; CONNECTION: FLANGE; BODY MATERIAL: STEEL; OPERATED: ELECTRIC; ENCLOSURE RATING: IP65; MEDIUM: BUTANE/NATURAL GAS/PROPANE; CURRENT: 0.33 A; OEM P/N: A2A50272850; SUPPL P/N: PB0000267703",null,"SOLENOID","DN25","STEEL","PN40",null,"FLANGE",null,null,"ELECTRIC","BUTANE/NATURAL GAS/PROPANE",null,"A2A50272850; PB0000267703","220 V; 0.33 A; IP65"]
["Gourikwa OCGT Power Station",622492,"VALVE, SOLENOID: PIPE SIZE: DN25; STYLE: 2/2; POTENTIAL: 230 V; DESIGN RATING: PN40; CONNECTION: FLANGE; BODY MATERIAL: STEEL; OPERATED: ELECTRIC; ENCLOSURE RATING: IP65; MEDIUM: BUTANE/NATURAL GAS/PROPANE; POWER: 160 W; CURRENT: 0.33 A; SPECIFICATION: DIN 3394-1; OEM P/N: 40-EVSADU 10NH-4 P.XN.09.20.32; SUPPL P/N: PB0000282466; A2A50296211","Uni Gerate","SOLENOID","DN25","STEEL","PN40",null,"FLANGE",null,null,"ELECTRIC","BUTANE/NATURAL GAS/PROPANE",null,"40-EVSADU 10NH-4 P.XN.09.20.32; PB0000282466","230 V; 160 W; 0.33 A; IP65"]
["Gourikwa OCGT Power Station",622742,"VALVE: TYPE: FUEL OIL TRANSFER; VALVE SIZE: G1/2 IN; TEMPERATURE RATING: MAX 140 DEG C; CONNECTION: FLANGE, FITTING; OPERATED: AUTOMATIC; BODY MATERIAL: STEEL; OEM P/N: A2A50323268; SUPPL P/N: PG0032860600",null,"FUEL OIL TRANSFER","G1/2 IN","STEEL",null,null,"FLANGE, FITTING",null,null,"AUTOMATIC",null,"MAX 140 DEG C","A2A50323268; PG0032860600"]
["Gourikwa OCGT Power Station",622743,"VALVE: TYPE: FUEL OIL PREMIX; VALVE SIZE: G1/2 IN; DESIGN RATING: PN100; TEMPERATURE RATING: MAX 160 DEG C; CONNECTION: FLANGE, FITTING; OPERATED: AUTOMATIC; BODY MATERIAL: STEEL; OEM P/N: A2A50328041; SUPPL P/N: PG0032863600",null,"FUEL OIL PREMIX","G1/2 IN","STEEL","PN100",null,"FLANGE, FITTING",null,null,"AUTOMATIC",null,"MAX 160 DEG C","A2A50328041; PG0032863600"]
["Gourikwa OCGT Power Station",626656,"VALVE, CHECK: TYPE: HYDRAULIC; VALVE SIZE: G1/2 IN; DESIGN RATING: MAX 350 BAR; TEMPERATURE RATING: -30 TO 80 DEG C; CONNECTION: G1/2 IN-BSPP; BODY MATERIAL: STEEL; FACE TO FACE LENGTH: 16 MM; OPERATED: PNEUMATIC; OEM P/N: PG0031832800; SUPPL P/N: A2A50315038",null,"CHECK; HYDRAULIC","G1/2 IN","STEEL","MAX 350 BAR",null,"G1/2 IN-BSPP","16 MM",null,"PNEUMATIC",null,"-30 TO 80 DEG C","PG0031832800; A2A50315038"]
["Gourikwa OCGT Power Station",643634,"VALVE: TYPE: CONTROL; VALVE SIZE: 6 IN; DESIGN RATING: 21 BAR; TEMPERATURE RATING: 65 DEG C; FACE TO FACE LENGTH: 235 MM; CONNECTION: WAFER; OPERATED: PILOT; BODY MATERIAL: CS; SPECIFICATION: 799-D; REFERENCE NO: 139163","INBAL","CONTROL","6 IN","CS","21 BAR",null,"WAFER","235 MM",null,"PILOT",null,"65 DEG C",139163]
["Gourikwa OCGT Power Station",644167,"VALVE: TYPE: STOP; VALVE SIZE: DN 50; DESIGN RATING: 16 BAR; TEMPERATURE RATING: 120 DEG C; FACE TO FACE LENGTH: 150 MM; CONNECTION: FLANGE; OPERATED: MANUAL; BODY MATERIAL: CAST IRON; GRADE: EN-JL1040; SPECIFICATION: ARI 12072; .",null,"STOP","DN 50","CAST IRON","16 BAR",null,"FLANGE","150 MM",null,"MANUAL",null,"120 DEG C"]
["Gourikwa OCGT Power Station",644168,"VALVE: TYPE: STOP; VALVE SIZE: DN 40; DESIGN RATING: 16 BAR; TEMPERATURE RATING: 120 DEG C; FACE TO FACE LENGTH: 140 MM; CONNECTION: FLANGE 150 MM; OPERATED: MANUAL; BODY MATERIAL: CAST IRON; GRADE: EN-JL1040; SPECIFICATION: ARI 12072",null,"STOP","DN 40","CAST IRON","16 BAR",null,"FLANGE 150 MM","140 MM",null,"MANUAL",null,"120 DEG C"]
["Gourikwa OCGT Power Station",644441,"VALVE: TYPE: CONTROL; VALVE SIZE: 2 IN; DESIGN RATING: 21 BAR; TEMPERATURE RATING: 65 DEG C; FACE TO FACE LENGTH: 190 MM; CONNECTION: FLANGE; OPERATED: PILOT; BODY MATERIAL: CS; SPECIFICATION: 711-D","INBAL","CONTROL","2 IN","CS","21 BAR",null,"FLANGE","190 MM",null,"PILOT",null,"65 DEG C"]
["Gourikwa OCGT Power Station",644442,"VALVE: TYPE: CONTROL; VALVE SIZE: 3 IN; DESIGN RATING: 21 BAR; TEMPERATURE RATING: 65 DEG C; FACE TO FACE LENGTH: 155 MM; CONNECTION: WAFER; OPERATED: PILOT; BODY MATERIAL: CARBON STL; SPECIFICATION: 799-D","INBAL","CONTROL","3 IN","CARBON STL","21 BAR",null,"WAFER","155 MM",null,"PILOT",null,"65 DEG C"]
["Gourikwa OCGT Power Station",644443,"VALVE: TYPE: CONTROL; VALVE SIZE: 4 IN; DESIGN RATING: 21 BAR; TEMPERATURE RATING: 65 DEG C; FACE TO FACE LENGTH: 187 MM; CONNECTION: WAFER; OPERATED: PILOT; BODY MATERIAL: CARBON STL; SPECIFICATION: 799-D","INBAL","CONTROL","4 IN","CARBON STL","21 BAR",null,"WAFER","187 MM",null,"PILOT",null,"65 DEG C"]
["Gourikwa OCGT Power Station",647831,"VALVE, BALL: VALVE SIZE: 1 IN; DESIGN RATING: 69 BAR; TEMPERATURE RATING: 50 DEG C; CONNECTION: BSP THREADED ENDS; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 88 MM; OPERATED: MANUAL; SOFTGOODS: PTFE; PORT TYPE: FULL BORE; GRADE: ASTM A351 GR CF8M; 2 PIECE SERIES 20",null,"BALL; FULL BORE","1 IN","STAINLESS STEEL","69 BAR",null,"BSP THREADED ENDS","88 MM",null,"MANUAL",null,"50 DEG C",null,null,"PTFE"]
["Gourikwa OCGT Power Station",647832,"VALVE, BALL: VALVE SIZE: 1/2 IN; DESIGN RATING: 69 BAR; TEMPERATURE RATING: 50 DEG C; CONNECTION: BSP THREADED ENDS; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 65 MM; OPERATED: MANUAL; SOFTGOODS: PTFE; PORT TYPE: FULL BORE; GRADE: ASTM A351 GR CF8M; 2 PIECE SERIES 20",null,"BALL; FULL BORE","1/2 IN","STAINLESS STEEL","69 BAR",null,"BSP THREADED ENDS","65 MM",null,"MANUAL",null,"50 DEG C",null,null,"PTFE"]
["Gourikwa OCGT Power Station",647833,"VALVE, BALL: VALVE SIZE: 3/4 IN; DESIGN RATING: 69; TEMPERATURE RATING: 50 DEG C; CONNECTION: BSP THREADED ENDS; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 74 MM; OPERATED: MANUAL; SOFTGOODS: PTFE; PORT TYPE: FULL BORE; GRADE: ASTM A351 GR CF8M; 2 PIECE SERIES 20",null,"BALL; FULL BORE","3/4 IN","STAINLESS STEEL",69,null,"BSP THREADED ENDS","74 MM",null,"MANUAL",null,"50 DEG C",null,null,"PTFE"]
["Gourikwa OCGT Power Station",650143,"VALVE, SOLENOID: PIPE SIZE: 3/4 IN; STYLE: 9 X CONNECTIONS; 3 X SOLENOID; POTENTIAL: 24 VDC; DESIGN RATING: 3 BAR; CONNECTION: BSP; BODY MATERIAL: BRASS; OPERATED: DIRECT SOLENOID; ENCLOSURE RATING: IP67; MEDIUM: WATER; POWER: 11.2 W; ORIFICE SIZE: 19 MM; COIL: DC; APPLICATION: CENTRIFUGE SEALING WATER; CLASSIFICATION: ZONE 2; SUPPL P/N: 176346680","Burkert","SOLENOID","DN15; 13 MM","BRASS","0.2-16 BAR",null,"PLUG",null,null,"DC V","AIR/WATER; GAS TURBINE FIRE SYSTEM",null,176346680,"24 VDC; 11.2 W; DC; IP67; ZONE 2"]
["Gourikwa OCGT Power Station",671840,"VALVE, SOLENOID: PIPE SIZE: DN15; STYLE: BLOCK; POTENTIAL: 24 VDC; DESIGN RATING: 0.2-16 BAR; CONNECTION: PLUG; BODY MATERIAL: BRASS; OPERATED: DC V; ENCLOSURE RATING: IP65; MEDIUM: AIR/WATER; POWER: 11 W; CURRENT: 0.46 A; ORIFICE SIZE: 13 MM; SOFTGOODS: SEAL NBR; APPLICATION: GAS TURBINE FIRE SYSTEM; SPECIFICATION: ISO; MANUF P/N: 840131",null,"SOLENOID","DN15; 13 MM","BRASS","0.2-16 BAR",null,"PLUG",null,null,"DC V","AIR/WATER; GAS TURBINE FIRE SYSTEM",null,840131,"24 VDC; 11 W; 0.46 A; IP65","SEAL NBR"]
["Gourikwa OCGT Power Station",671894,"VALVE: TYPE: CHANGE OVER; VALVE SIZE: 1-1/2 IN; DESIGN RATING: 40-100 BAR; TEMPERATURE RATING: -10 TO 425 DEG C; FACE TO FACE LENGTH: 265 MM; CONNECTION: DN 40; OPERATED: HAND; BODY MATERIAL: GP 240GM + N 1.0619; STYLE: CHANGE OVER VALVE; TRIM: CR 1,4021; GRADE: CARBON STEEL; SOFTGOODS: GRAPHITE/1,4571; SPECIAL FEATURES: CHANGE OVER VALVE,3 PORTS FLANGE; PN - 300 LBS","Leser","3 PORTS FLANGE; CHANGE OVER","1-1/2 IN","GP 240GM + N 1.0619","40-100 BAR","CR 1,4021","DN 40","265 MM",null,"HAND",null,"-10 TO 425 DEG C",null,null,"GRAPHITE/1,4571"]
["Gourikwa OCGT Power Station",708469,"VALVE: TYPE: DELUGE; VALVE SIZE: 3 IN; DESIGN RATING: 21 BAR; TEMPERATURE RATING: 65 DEG C; CONNECTION: WAFER; OPERATED: ACTUATOR HYDRAULIC; BODY MATERIAL: FORGED STEEL SAE1021; INBAL MODEL 799DG-04-A01 HYDRAULIC DELGE VALVE- WAGER PATTERN ENDS RATED TO 21 TO OPEN WHEN PRESSURE IS LOST IN THE LINE, LATCH IN OPEN POSITION, LOCAL RESET COMPLETE WITH ALL NECESSARY TRIM VALVE ENDS AND WATER FLOW TEST & DRAIN ENDS DUCTILE (ASTM A53665-45-12), SLEEVE SMR5 ELATOMER REINFORCED WITH POLYESTER AND KEVLAR, CONTROL TRIM BRASS NICKEL CHROME PLATED STAINLESS STEEL AND GALVANISED STEEL","INBAL","DELUGE","3 IN","FORGED STEEL SAE1021","21 BAR",null,"WAFER",null,null,"ACTUATOR HYDRAULIC",null,"65 DEG C"]
["Gourikwa OCGT Power Station",708473,"VALVE: TYPE: DELUGE; VALVE SIZE: 4 IN; DESIGN RATING: 21 BAR; TEMPERATURE RATING: 65 DEG C; CONNECTION: WAFER; OPERATED: ACTUATOR HYDRAULIC; BODY MATERIAL: FORGED STEEL SAE1021; INBAL MODEL 799DG-04-A01 HYDRAULIC DELGE VALVE- WAGER PATTERN ENDS RATED TO 21 TO OPEN WHEN PRESSURE IS LOST IN THE LINE, LATCH IN OPEN POSITION, LOCAL RESET COMPLETE WITH ALL NECESSARY TRIM VALVE ENDS AND WATER FLOW TEST & DRAIN ENDS DUCTILE (ASTM A53665-45-12), SLEEVE SMR5 ELATOMER REINFORCED WITH POLYESTER AND KEVLAR, CONTROL TRIM BRASS NICKEL CHROME PLATED STAINLESS STEEL AND GALVANISED STEEL","INBAL","DELUGE","4 IN","FORGED STEEL SAE1021","21 BAR",null,"WAFER",null,null,"ACTUATOR HYDRAULIC",null,"65 DEG C"]
["Gourikwa OCGT Power Station",758582,"VALVE: TYPE: NRV; VALVE SIZE: 3/8 IN; DESIGN RATING: 700 BAR; TEMPERATURE RATING: 0 to 80 DEG; FACE TO FACE LENGTH: 11.7 MM; CONNECTION: THREAD 1/4 INCH BSP; OPERATED: BALL, SPRING; BODY MATERIAL: STAINLESS STEEL; STYLE: 1 WAY; SPECIFICATION: HAWE HYDRAULICS RB2 NRV SIZE: 3/8” BSPP; SOFTGOODS: 0-RINGS, SPRINGS; SPECIAL FEATURES: HAWE HYDRAULICS RB2 NRV SIZE: 3/8” BSPP","Hawe","NRV","3/8 IN","STAINLESS STEEL","700 BAR",null,"THREAD 1/4 INCH BSP","11.7 MM",null,"BALL, SPRING",null,"0 to 80 DEG",null,null,"0-RINGS, SPRINGS"]
["Gariep Hydro Power Station",71418,"VALVE, GATE: VALVE SIZE: 250 MM; TYPE: SOLID WEDGE; DESIGN PRESSURE: 10 BAR; DESIGN TEMPERATURE: 0-100 DEG C; CONNECTION: FLANGE; FACE TO FACE LENGTH: 325 MM; BODY MATERIAL: STEEL CAST; TRIM: BONNET/DISC STEEL; OPERATED: HANDWHEEL; STEM DESIGN: RISING OS; STYLE: BOLTED BONNET; DESIGN RATING: 10 BAR; REFERENCE NO: FBS10K250; PCD","FUJI","GATE; SOLID WEDGE","250 MM","STEEL CAST","10 BAR","BONNET/DISC STEEL; RISING OS","FLANGE","325 MM",null,"HANDWHEEL",null,"0-100 DEG C","FBS10K250"]
["Gariep Hydro Power Station",688633,"VALVE: TYPE: KNIFE GATE; VALVE SIZE: 450 MM; DESIGN RATING: 7 BAR; TEMPERATURE RATING: 50 DEG C; FACE TO FACE LENGTH: 143 MM; CONNECTION: FLANGE; OPERATED: HYDRAULIC ACTUATOR; BODY MATERIAL: CS; 16-HOLE EQUI-SPACED, OFF CRS ON A 585 PCD; 10-HOLES DRILL DIAMETER 26 THRU; 6-HOLES DRILL AND TAP M24 X 30 DEEP","PV ENGINEERING","KNIFE GATE","450 MM","CS","7 BAR",null,"FLANGE","143 MM","16-HOLE EQUI-SPACED, OFF CRS ON A 585 PCD","HYDRAULIC ACTUATOR",null,"50 DEG C"]
["Gariep Hydro Power Station",754499,"VALVE, CHECK: TYPE: CHECK VALVE; VALVE SIZE: ¼ BSPT MALE DOWNSTREAM / 8L MALE UPSTREAM IN; DESIGN RATING: 500 BAR; TEMPERATURE RATING: -10 to +100 DEG C; CONNECTION: ¼ INCH BSPT MALE DOWNSTREAM / 8L MALE UPSTREAM; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 47.5 MM; OPERATED: PRESSURE; STYLE: HYDRAULIC; TRIM: STELLITED; APPLICATION: GREASE SYSTEM; SPECIFICATION: RHZ-R-ED",null,"CHECK; CHECK VALVE","¼ BSPT MALE DOWNSTREAM / 8L MALE UPSTREAM IN","STAINLESS STEEL","500 BAR","STELLITED","¼ INCH BSPT MALE DOWNSTREAM / 8L MALE UPSTREAM","47.5 MM",null,"PRESSURE","GREASE SYSTEM","-10 to +100 DEG C"]
["Drakensberg Pumped Storage Scheme",43262,"VALVE: TYPE: SUCTION; VALVE SIZE: 144 MM; CONNECTION: COMPRESSION; OPERATED: PRESSURE; BODY MATERIAL: STAINLESS STEEL; TRIM: DISC STL; REFERENCE NO: HT303811; 2ND STAGE; 20P-4PORTS; 46.3MM THK PLATE; 88MM THK O/A; WITH HEX NUT, WASHER AND SPLIT PIN","Burckhardt Compression","SUCTION","144 MM","STAINLESS STEEL","150-600 Psi","DISC STL","COMPRESSION","3T size: 144 mm; connection: compression; operated: pressure; body material: stainless steel; trim: disc stl; reference no: ht303811","N/S","PRESSURE","AIR/OIL/WATER;","−196 to +538 deg","HT303811"]
["Drakensberg Pumped Storage Scheme",43264,"VALVE: TYPE: SUCTION; VALVE SIZE: 104 MM; CONNECTION: COMPRESSION; OPERATED: PRESSURE; BODY MATERIAL: STAINLESS STEEL; TRIM: DISC STL; REFERENCE NO: HT303815; 4TH STAGE; 20P-2PORTS; 46.3MM THK PLATE; 89MM THK O/A; WITH HEX NUT, WASHER AND SPLIT PIN","Burckhardt Compression","SUCTION","104 MM","STAINLESS STEEL","N/A","DISC STL","COMPRESSION","3T size: 104 mm; connection: compression; operated: pressure; body material: stainless steel; trim: disc stl; reference no: ht303815","N/S","PRESSURE","AIR/OIL/WATER;","up to 120 deg","HT303815"]
["Drakensberg Pumped Storage Scheme",43264,"VALVE: TYPE: SUCTION; VALVE SIZE: 104 MM; CONNECTION: COMPRESSION; OPERATED: PRESSURE; BODY MATERIAL: STAINLESS STEEL; TRIM: DISC STL; REFERENCE NO: HT303815; 4TH STAGE; 20P-2PORTS; 46.3MM THK PLATE; 89MM THK O/A; WITH HEX NUT, WASHER AND SPLIT PIN","Burckhardt Compression","SUCTION","104 MM","STAINLESS STEEL","N/A","DISC STL","COMPRESSION","3T size: 104 mm; connection: compression; operated: pressure; body material: stainless steel; trim: disc stl; reference no: ht303815","N/S","PRESSURE","AIR/OIL/WATER;","up to 120 deg","HT303815"]
["Drakensberg Pumped Storage Scheme",43264,"VALVE: TYPE: SUCTION; VALVE SIZE: 104 MM; CONNECTION: COMPRESSION; OPERATED: PRESSURE; BODY MATERIAL: STAINLESS STEEL; TRIM: DISC STL; REFERENCE NO: HT303815; 4TH STAGE; 20P-2PORTS; 46.3MM THK PLATE; 89MM THK O/A; WITH HEX NUT, WASHER AND SPLIT PIN","Burckhardt Compression","SUCTION","104 MM","STAINLESS STEEL","N/A","DISC STL","COMPRESSION","3T size: 104 mm; connection: compression; operated: pressure; body material: stainless steel; trim: disc stl; reference no: ht303815","N/S","PRESSURE","AIR/OIL/WATER;","up to 120 deg","HT303815"]
["Drakensberg Pumped Storage Scheme",43265,"VALVE: TYPE: DISCHARGE; VALVE SIZE: 164 MM; CONNECTION: COMPRESSION; OPERATED: PRESSURE; BODY MATERIAL: STAINLESS STEEL; TRIM: DISC STL; REFERENCE NO: HT303810; ASSY; 1ST STAGE 20P- 5PORTS; 46.0MM THK PLATE; 70MM THK O/A; WITH HEX NUT AND SPLIT PIN","Burckhardt Compression","DISCHARGE","164 MM","STAINLESS STEEL","N/A","DISC STL","COMPRESSION","3 ve size: 164 mm; connection: compression; operated: pressure; body material: stainless steel; trim: disc stl; reference no: ht303810","N/S","PRESSURE","AIR/OIL/WATER;","80-120 deg","HT303810"]
["Drakensberg Pumped Storage Scheme",62413,"VALVE, SOLENOID: PIPE SIZE: 12 MM; STYLE: 4 WAY; POTENTIAL: 240 - 250 VDC; DESIGN RATING: 70-700 KPA; CONNECTION: FNPT; BODY MATERIAL: BRASS; OPERATED: PRESSURE; ENCLOSURE RATING: IP65 EN 60529; MEDIUM: AIR/OIL/WATER; POWER: 11.2 W; APPLICATION: BLOWDOWN COMPRESSOR; REFERENCE NO: WP8345E001; GENERAL PURPOSE ENCLOSURE; 240 VDC COIL","ASCO Numatics","SOLENOID","12 MM","BRASS","70-700 KPA","SS spool & armature with NBR seals and PTFE guide rings","FNPT","95 mm","N/S","PRESSURE","AIR/OIL/WATER; BLOWDOWN COMPRESSOR","80 deg","WP8345E001","240 - 250 VDC; 11.2 W; IP65 EN 60529"]
["Drakensberg Pumped Storage Scheme",63152,"VALVE, GATE: VALVE SIZE: 3/4 IN; TYPE: SOLID WEDGE; CONNECTION: FLANGE; BODY MATERIAL: BRASS; TRIM: DISC BRS; OPERATED: HANDWHEEL; STEM DESIGN: INSIDE SCREW; STYLE: THD BONNET; NEEDLE VALVE; FLANGE SIZE 105MM O/D; 4 HOLES 14MM DIA PCD 75MM; BS 2060","Bristol Valves","GATE; SOLID WEDGE","3/4 IN","BRASS","N/A","DISC BRS; INSIDE SCREW","FLANGE","5; mm","75MM; 4 HOLES 14MM DIA PCD 75MM","HANDWHEEL","AIR/OIL/WATER;","up to 200 deg"]
["Drakensberg Pumped Storage Scheme",63348,"VALVE, BALL: VALVE SIZE: 3/4 IN; DESIGN RATING: 1000 KPA; CONNECTION: FEMALE THD; OPERATED: LEVER; STYLE: 3 WAY; 3 PIECE; TRIM: BALL SS GR 316; SOFTGOODS: SEALS PTFE; GRADE: CF8M; ACID WATER OIL AND GAS; THROUGHWAY IN BALL TO BE 20 MM","Parker Hannifin","BALL","3/4 IN","MEEAL","1000 KPA","BALL SS GR 316","FEMALE THD","334 in","N/S","LEVER","Acid Water, Oil and Gas","5-100 deg",null,null,"SEALS PTFE"]
["Drakensberg Pumped Storage Scheme",65786,"VALVE, GATE: VALVE SIZE: 250 MM; TYPE: SPHERICAL MANUAL BYPASS; CONNECTION: FLANGE; FACE TO FACE LENGTH: 250 MM; BODY MATERIAL: STEEL; OPERATED: HANDWHEEL; TEMPERATURE RATING: 16 DEG C; DESIGN RATING: 7.2 MPA; MAIN BY-PASS VALVE VOEST-ALPINE TYPE MB9-642-5320A ESKOM NO. 0.48/1121 DESIGNE PRESSURE = 7.2 MPA VALVE, BYPASS MAIN 5320 A","MB9-642-5320A","GATE; BYPASS MAIN 5320 A; SPHERICAL MANUAL BYPASS","250 MM","STEEL","7.2 MPA","13Cr/Alloy steel spherical wedge, Stellite hard-faced seats, SS stem, graphite packing","FLANGE","250 MM","N/S","HANDWHEEL","WATER","16 DEG C"]
["Drakensberg Pumped Storage Scheme",65917,"VALVE, RELIEF: VALVE SIZE: 45 X 40 MM; SET PRESSURE: 70 BAR; CONNECTION: NPT X FNPT; BODY MATERIAL: STL; TRIM: DISC/SPRING STL; OPERATED: PRESSURE, SPRING; SAFETY","Bopp & Reuther","RELIEF","45 X 40 MM","STL","70 BAR","DISC/SPRING STL","NPT X FNPT","N/S","N/S","PRESSURE, SPRING","AIR,WATER,OIL","up to 425 deg"]
["Drakensberg Pumped Storage Scheme",66072,"VALVE, CHECK: TYPE: PISTON; VALVE SIZE: 25 MM; CONNECTION: NPT; BODY MATERIAL: STAINLESS STEEL; STYLE: THD CAP; TRIM: DISC/CAP STL; NON-RETURN; EO; TUBE SIZE 25MM OD EO TUBE CONNECTION AT BOTH ENDS","Parker Hannifin","CHECK; PISTON","25 MM","STAINLESS STEEL","N/S","DISC/CAP STL","NPT","190 mm","N/S","Hydraulic/tube system service","oil, hydraulic fluid, gas","−196 to +538 deg"]
["Drakensberg Pumped Storage Scheme",66074,"VALVE, BALL: VALVE SIZE: 16 MM; DESIGN RATING: 100 BAR; TEMPERATURE RATING: -200 TO 200 DEG C; CONNECTION: NPT X FNPT; BODY MATERIAL: STEEL; OPERATED: LEVER; STYLE: 4 WAY; TRIM: BALL STL; SPECIFICATION: DIN 3230; PORT TYPE: 3 X MALE; 1 X FEMALE; APPLICATION: UPSTREAM SEAL CHANGE OVER VALVE; TYPE: MANUAL OPERATED; SUPPL P/N: 1017489; REFERENCE NO: 1017489; 3 MALE X 1 FEMALE; CHANGE-OVER; BLOCK; ARGUS","Argus","BALL; 3 X MALE; MANUAL OPERATED","16 MM","STEEL","100 BAR","BALL STL","NPT X FNPT","95 mm","N/S","LEVER","UPSTREAM SEAL CHANGE OVER VALVE","-200 TO 200 DEG C",1017489]
["Drakensberg Pumped Storage Scheme",66205,"VALVE, RELIEF: SET PRESSURE: 60 BAR; REFERENCE NO: MB8-222-2450C60B; SAFETY","Burckhardt Compression","RELIEF","N/S","STEEL","60 BAR","SS disc & seat, SS spindle, chrome alloy spring (metal-seated safety valve)","TBC","N/S","N/S","PRESSURE","Safety Protection","180 deg","MB8-222-2450C60B"]
["Drakensberg Pumped Storage Scheme",66232,"VALVE, DIAPHRAGM: VALVE SIZE: 15 MM; CONNECTION: FNPT; BODY MATERIAL: CI; DIAPHRAGM MATERIAL: RUBBER GR Q; OPERATED: HANDWHEEL; STYLE: WEIR; REFERENCE NO: A; SAUNDERS","Saunders","DIAPHRAGM","15 MM","CI; RUBBER GR Q","N/S","RUBBER GR Q","FNPT","A6 fnpt","N/S","HANDWHEEL","Water, slurry, or compatible process fluid","20-90 deg","A"]
["Drakensberg Pumped Storage Scheme",66529,"VALVE, CHECK: TYPE: SWING; VALVE SIZE: 400 MM; DESIGN RATING: 16 BAR; CONNECTION: FLANGE; BODY MATERIAL: CS; TRIM: BONNET/DISC STEEL; REFERENCE NO: 16SMZ; CHECKRITE NON-RETURN; HYDRO. TEST CERTIFICATE REQUIRED FOR ALL VALVES","Check-Rite Valves","CHECK; SWING","400 MM","CS","16 BAR","BONNET/DISC STEEL","FLANGE","6:valve size: 400 mm; design rating: 16 bar; connection: flange","N/S","PRESSURE","Process fluid service","150 deg","16SMZ",null,null,"CERTIFICATE REQUIRED FOR ALL VALVES"]
["Drakensberg Pumped Storage Scheme",66535,"VALVE, BALL: VALVE SIZE: 1/2 IN; DESIGN RATING: 40 LB; TEMPERATURE RATING: 25 DEG C; CONNECTION: FNPT; BODY MATERIAL: STAINLESS STEEL; OPERATED: LEVER; STYLE: UNION BONNET; TRIM: BALL SS; BRASS; WITH FIXED FEMALE FLANGE EITHER END","Swagelok","BALL","1/2 IN","STAINLESS STEEL","40 LB","BALL SS","FNPT","N/S","N/S","LEVER","General process/instrument service","25 DEG C"]
["Drakensberg Pumped Storage Scheme",68148,"VALVE, RELIEF: VALVE SIZE: 50 MM; SET PRESSURE: 35 KPA; CONNECTION: THD; BODY MATERIAL: STL; TRIM: BRASS; OPERATED: SPRING; PRESSURE RANGE: 2-20 LB; REFERENCE NO: MD0014; SAFETY; TYPE 616-2; TYPE: HLP","Hale Hamilton","RELIEF; HLP","50 MM","STL","2-20 LB; 35 KPA","BRASS","THD","100 mm","N/S","SPRING","Pressure relief service","80 deg","MD0014"]
["Drakensberg Pumped Storage Scheme",70478,"VALVE, RELIEF: VALVE SIZE: 50 X 32 MM; SET PRESSURE: 600 KPA; TEMPERATURE RATING: -10 TO 14 DEG C; CONNECTION: FLANGE; BODY MATERIAL: CI; TRIM: STAINLESS STEEL; OPERATED: PRESSURE; DESIGN RATING: 16 BAR; PRESSURE RANGE: 6 BAR; FIG NO: 4411/H2; REFERENCE NO: 16; SAFETY; INLET AND OUTLET PN16; TO SIZED TO DIN3320 AND TEST APPROVED IN ACCORDANCE WITH (AD-MERKBLATT A2); FLOW CAPACITY TO BE AT LEAST 35000 KG/HR","HEROSE","RELIEF","50 X 32 MM","CI","16 BAR; 6 BAR; 600 KPA","STAINLESS STEEL","FLANGE","95 mm","N/S","PRESSURE","Pressure relief service","-10 TO 14 DEG C","16; 4411/H2"]
["Drakensberg Pumped Storage Scheme",72012,"VALVE, BALL: VALVE SIZE: 50 MM; DESIGN RATING: 6 BAR; CONNECTION: FLANGE; BODY MATERIAL: STEEL; OPERATED: LEVER; STYLE: 2 WAY; TRIM: BALL STL; BOHMER; SERIES FK","Bohmer","BALL","50 MM","STEEL","6 BAR","BALL STL","FLANGE","95 mm","N/S","LEVER","Process fluid service","150 deg"]
["Drakensberg Pumped Storage Scheme",72040,"VALVE, GATE: VALVE SIZE: 3 IN; TYPE: SOLID WEDGE; CONNECTION: FLANGE; BODY MATERIAL: STEEL; TRIM: SEAT 13CR; OPERATED: HANDWHEEL; STEM DESIGN: RISING OUTSIDE SCREW; STYLE: BOLTED BONNET; GRADE: WCB; DESIGN RATING: 150 LB; REFERENCE NO: 2H27347; CAST; HIRATA","Hirata","GATE; SOLID WEDGE","3 IN","STEEL","150 LB","SEAT 13CR; RISING OUTSIDE SCREW","FLANGE","210 mm","N/S","HANDWHEEL","Isolation service","200 deg","2H27347",null,"R"]
["Drakensberg Pumped Storage Scheme",72046,"VALVE, GATE: VALVE SIZE: 2-1/2 IN; CONNECTION: FLANGE; BODY MATERIAL: CS; DESIGN RATING: 150 LB; DRAWING NO: 2H27346 REV 1","Hopkinsons Valve (probable)","GATE","2-1/2 IN","CS","150 LB","N/S","FLANGE","190 mm","N/S","HANDWHEEL","Isolation service","200 deg","2H27346 REV 1"]
["Drakensberg Pumped Storage Scheme",72057,"VALVE, GATE: VALVE SIZE: 100 MM; CONNECTION: FLANGE; BODY MATERIAL: CS; DESIGN RATING: 150 LB; REFERENCE NO: 2H27354; HIRATA","Hirata","GATE","100 MM","CS","150 LB","N/S","FLANGE","230 mm","N/S","HANDWHEEL","Isolation service","200 deg","2H27354"]
["Drakensberg Pumped Storage Scheme",72058,"VALVE, GATE: VALVE SIZE: 3/8 IN; TYPE: SOLID WEDGE; CONNECTION: FNPT; BODY MATERIAL: STEEL; TRIM: SEAT 13CR; OPERATED: HANDWHEEL; STEM DESIGN: RISING OUTSIDE SCREW; STYLE: BOLTED BONNET; DESIGN RATING: 600 LB; DRAWING NO: 2N27361 REV 1; FORGED; HIRATA","Hirata","GATE; SOLID WEDGE","3/8 IN","STEEL","600 LB","SEAT 13CR; RISING OUTSIDE SCREW","FNPT","260 mm","N/S","HANDWHEEL","Isolation service","350 deg","2N27361 REV 1",null,"R"]
["Drakensberg Pumped Storage Scheme",72060,"VALVE, GLOBE: VALVE SIZE: 10 MM; OPERATED: HANDWHEEL; CONNECTION: FNPT; BODY MATERIAL: SS FORGED; TRIM: SEAT 13CR; STEM DESIGN: RISING OUTSIDE SCREW; STYLE: BOLTED BONNET; DESIGN RATING: 150 LB; DRAWING NO: 2S18670 REV 1; 3/8 INCH; HIRATA","Hirata","GLOBE","10 MM","SS FORGED","150 LB","SEAT 13CR; RISING OUTSIDE SCREW","FNPT","N/S","N/S","HANDWHEEL","Isolation/control service","300 deg","2S18670 REV 1",null,"R"]
["Drakensberg Pumped Storage Scheme",72062,"VALVE, GLOBE: VALVE SIZE: 1/2 IN; OPERATED: HANDWHEEL; CONNECTION: FLANGE; BODY MATERIAL: STL FORGED; TRIM: SEAT 13CR; STEM DESIGN: INSIDE SCREW; STYLE: BOLTED BONNET; DESIGN RATING: 150-800 LB; DRAWING NO: 2M18627 REV 1; HIRATA","Hirata","GLOBE","1/2 IN","STL FORGED","150-800 LB","SEAT 13CR; INSIDE SCREW","FLANGE","108 mm","N/S","HANDWHEEL","Isolation/control service","−29 to 425 deg","2M18627 REV 1",null,"R"]
["Drakensberg Pumped Storage Scheme",73053,"VALVE, BUTTERFLY: TYPE: WAFER; VALVE SIZE: 75 MM; DESIGN RATING: 740 LB; TEMPERATURE RATING: -250 TO 500 DEG F; CONNECTION: FLANGE; BODY MATERIAL: STAINLESS STEEL; TRIM: DISC SS GR 316; ELECTRICAL; MINITORK ASSY TURB","Minitork (actuator/assembly)","BUTTERFLY; WAFER","75 MM","STAINLESS STEEL","740 LB","DISC SS GR 316","FLANGE","43 mm","N/S","HANDWHEEL","Isolation/throttling service","-250 TO 500 DEG F"]
["Drakensberg Pumped Storage Scheme",77118,"VALVE, RELIEF: VALVE SIZE: 1/4 IN; SET PRESSURE: 60 LB; CONNECTION: NPT; BODY MATERIAL: BRASS; TRIM: SPRING STL; STEM BRS; OPERATED: PRESSURE, SPRING; SUPPL P/N: 3W123 662T2; STOP","Haskel Energy Systems (probable)","RELIEF","1/4 IN","BRASS","60 LB","SPRING STL","NPT","50 mm","N/S","PRESSURE, SPRING","Pressure relief / stop service","−29 to 200 deg","3W123 662T2"]
["Drakensberg Pumped Storage Scheme",77124,"VALVE: TYPE: DISCHARGE; VALVE SIZE: 27 MM; CONNECTION: COMPRESSION; OPERATED: PRESSURE; BODY MATERIAL: STL; TRIM: DISC STL; REFERENCE NO: 30279459","Burckhardt Compression","DISCHARGE","27 MM","STL","N/S","DISC STL","COMPRESSION","7 ve size: 27 mm","N/S","PRESSURE","Air compressor discharge service","150–200 deg",30279459]
["Drakensberg Pumped Storage Scheme",77134,"VALVE, RELIEF: VALVE SIZE: 1/4 IN; SET PRESSURE: 1300 LB; CONNECTION: NPT; BODY MATERIAL: BRASS; TRIM: SPRING STL; OPERATED: PRESSURE, SPRING; MODEL NO: 15T2; REFERENCE NO: X1396T19-1300; SAFETY; FOR TYPE 30; ING-RAND COMPRESSOR","Ing-Rand","RELIEF","1/4 IN","BRASS","1300 LB","SPRING STL","NPT","55 mm","N/S","PRESSURE, SPRING","Air compressor safety relief service","−29 to 200 deg","X1396T19-1300; 15T2"]
["Drakensberg Pumped Storage Scheme",77142,"VALVE, RELIEF: VALVE SIZE: 1/4 IN; SET PRESSURE: 1300 LB; CONNECTION: NPT; BODY MATERIAL: BRASS; TRIM: SPRING STL; STEM BRS; OPERATED: PRESSURE, SPRING; REFERENCE NO: W123662T2; SAFETY; ING-RAND","Ing-Rand","RELIEF","1/4 IN","BRASS","1300 LB","SPRING STL","NPT","N/S","N/S","PRESSURE, SPRING","Air compressor safety relief service","N/S","W123662T2"]
["Drakensberg Pumped Storage Scheme",77155,"VALVE, SOLENOID: PIPE SIZE: 10 MM; STYLE: 5 WAY; POTENTIAL: 220 VAC; DESIGN RATING: 315 BAR; BODY MATERIAL: STEEL; MEDIUM: OIL; REFERENCE NO: S10G51G020001100; 35 HZ; CONNECTION MANIFOLD; GENERAL PURPOSE ENCLOSURE; PUMP PILOT VALVE","Maximator","SOLENOID","10 MM","STEEL","315 BAR","N/S","Manifold mounted","190 mm","N/S","Solenoid actuated","OIL","N/S","S10G51G020001100","220 VAC"]
["Drakensberg Pumped Storage Scheme",77157,"VALVE: TYPE: EXHAUST; VALVE SIZE: 15 MM; CONNECTION: THD FEMALE; OPERATED: PRESSURE; BODY MATERIAL: ALUMINIUM; STYLE: 3 WAY; TRIM: BONNET AL; REFERENCE NO: 3340 B 10 HD-D6461; SCHOVILL SCHREIDER QUICK SHUTTLE VALVES","Schovill Schreider","EXHAUST","15 MM","ALUMINIUM","Ref. 3340 B 10 HD-D6461","BONNET AL","THD FEMALE","100 size","N/S","PRESSURE","Pneumatic exhaust/control service","N/S","3340 B 10 HD-D6461"]
["Drakensberg Pumped Storage Scheme",77165,"VALVE, BALL: VALVE SIZE: 25 MM; DESIGN RATING: 315 LB; CONNECTION: FNPT; BODY MATERIAL: STEEL; OPERATED: LEVER; STYLE: 2 WAY; BOHMER BLOCK","Bohmer","BALL","25 MM","STEEL","315 LB","N/S","FNPT","95 mm","N/S","LEVER","Isolation service","N/S"]
["Drakensberg Pumped Storage Scheme",77169,"VALVE, GATE: VALVE SIZE: 100 MM; TYPE: SOLID WEDGE; CONNECTION: FLANGE; BODY MATERIAL: STEEL; TRIM: BONNET STL; OPERATED: HYDRAULIC; STEM DESIGN: RISING OUTSIDE SCREW; STYLE: BOLTED BONNET; DESIGN RATING: 150 LB; REFERENCE NO: 20WRC; RUNNER COOLING WATER SUPPLY AUTO","Hopkinsons Valve","GATE; SOLID WEDGE","100 MM","STEEL","150 LB","BONNET STL; RISING OUTSIDE SCREW","FLANGE","710 rilling / PCD, Mediumrilling / PCD, Medium","N/S","HYDRAULIC","Runner cooling water supply","N/S","20WRC"]
["Drakensberg Pumped Storage Scheme",77200,"VALVE: TYPE: SUCTION; VALVE SIZE: 167 MM; CONNECTION: COMPRESSION; OPERATED: PRESSURE; BODY MATERIAL: STL; TRIM: DISC STL; REFERENCE NO: HT303809; 1ST STAGE","CLA-VAL","SUCTION","167 MM","STL","Ref. HT303809","DISC STL","COMPRESSION","7D size: 167 mm; connection: compression","N/S","PRESSURE","Compressed gas suction service","typically ~−20 °C to +60 °C suction conditions, up to ~120 °C depending on compressor design and OEM limits HT303809","HT303809"]
["Drakensberg Pumped Storage Scheme",77201,"VALVE: TYPE: DISCHARGE; VALVE SIZE: 145 MM; CONNECTION: COMPRESSION; OPERATED: PRESSURE; BODY MATERIAL: STL; TRIM: DISC STL; REFERENCE NO: HT303812; ASSEMBLY; 2ND STAGE","CLA-VAL","DISCHARGE","145 MM","STL","Ref. HT303812","DISC STL","COMPRESSION","7:ve size: 145 mm; connection: compression; operated: pressure","N/S","PRESSURE","Compressed gas discharge service","−20 °C to +160 °C","HT303812"]
["Drakensberg Pumped Storage Scheme",77202,"VALVE: TYPE: DISCHARGE; VALVE SIZE: 103.7 MM; DESIGN RATING: 0-250 DEG C; TEMPERATURE RATING: 0-250 DEG C; CONNECTION: COMPRESSION; OPERATED: PRESSURE; BODY MATERIAL: STL; TRIM: DISC STL; REFERENCE NO: HT303814; ASSEMBLY; 3RD STAGE","CLA-VAL","DISCHARGE","103.7 MM","STL","0-250 DEG C","DISC STL","COMPRESSION","N/S","N/S","PRESSURE","3rd stage discharge service","0-250 DEG C","HT303814"]
["Drakensberg Pumped Storage Scheme",77203,"VALVE: TYPE: DISCHARGE; VALVE SIZE: 104.4 MM; CONNECTION: COMPRESSION; OPERATED: PRESSURE; BODY MATERIAL: STL; TRIM: DISC STL; REFERENCE NO: HT303816; ASSEMBLY; 4TH STAGE","CLA-VAL","DISCHARGE","104.4 MM","STL","Ref. HT303812","DISC STL","COMPRESSION","7Ive size: 104.4 mm; connection: compression; operated: pressure","N/S","PRESSURE","High-pressure compressed gas discharge service","N/A","HT303816"]
["Drakensberg Pumped Storage Scheme",77242,"VALVE, ANGLE: TYPE: GLOBE; VALVE SIZE: 100 MM; DESIGN RATING: 600 LB; CONNECTION: FLANGE; BODY MATERIAL: STL; OPERATED: HYDRAULIC; STYLE: BOLTED BONNET; TRIM: BONNET/STEM STL; DRAWING NO: M-6WO78AG8 REV 1; REFERENCE NO: 20DA1/2; AIR ADMISSION; FOR TAIL WATER DEPRESSING","CLA-VAL","ANGLE; GLOBE","100 MM","STL","600 LB","BONNET/STEM STL","FLANGE","95 mm","N/S","HYDRAULIC","Air admission service","N/S","20DA1/2; M-6WO78AG8 REV 1"]
["Drakensberg Pumped Storage Scheme",178035,"VALVE, RELIEF: REFERENCE NO: 0523C","KITZ Corporation","RELIEF","1/2 IN AND 3/4 IN","STEEL","N/S","N/S","TBC","N/S","N/S","PRESSURE","Pressure relief / safety protection service","N/S","0523C"]
["Drakensberg Pumped Storage Scheme",401291,"VALVE, BALL: VALVE SIZE: 3/4 IN; OPERATED: HANDLE; TYPE: STOP","KITZ Corporation/Apollo Valves","BALL; STOP","3/4 IN","STEAL","N/S","N/S","TBC","95 in","N/S","HANDLE","Isolation service","N/S"]
["Drakensberg Pumped Storage Scheme",403617,"VALVE, RELIEF: APPLICATION: LATCO PRESSURE CONTROL; DESIGN RATING: 400 KPA","LATCO","RELIEF","N/S","STEEL","400 KPA","N/S","TBC","129 mm","N/S","Pressure operated (automatic)","LATCO PRESSURE CONTROL","20-80 deg"]
["Drakensberg Pumped Storage Scheme",502387,"VALVE: TYPE: COMPRESSOR 3RD STAGE; OPERATED: AUTOMATIC; BODY MATERIAL: STL; SUPPL P/N: 31517725","Atlas Copco","COMPRESSOR 3RD STAGE","20 GA","STL","N/S","N/S","COMPRESSION","N/S","N/S","AUTOMATIC","Compressed air service","N/S",31517725]
["Drakensberg Pumped Storage Scheme",502388,"VALVE: TYPE: COMPRESSOR 2ND STAGE; OPERATED: AUTOMATIC; BODY MATERIAL: STL; SUPPL P/N: 37004827","Atlas Copco","COMPRESSOR 2ND STAGE","35 GA","STL","N/S","N/S","COMPRESSION","N/S","N/S","AUTOMATIC","Compressed air service","N/S",37004827]
["Drakensberg Pumped Storage Scheme",502396,"VALVE: TYPE: 1ST STAGE; VALVE SIZE: 164MM X 85 IN; TEMPERATURE RATING: 0-250 DEG C; CONNECTION: COMPRESSION; OPERATED: AUTOMATIC; BODY MATERIAL: STEEL; MANUF P/N: 37101946","Atlas Copco","1ST STAGE","164MM X 85 IN","STEEL","N/S","N/S","COMPRESSION","2Ave size: 164mm x 85 in","N/S","AUTOMATIC","Compressed air / process gas service","0-250 DEG C",37101946]
["Drakensberg Pumped Storage Scheme",640478,"VALVE, GLOBE: VALVE SIZE: 2 IN; DESIGN PRESSURE: 102 BAR; DESIGN TEMPERATURE: -29 TO 38 DEG C; FACE TO FACE LENGTH: 292.1 MM; OPERATED: HANDWHEEL, MANUAL; CONNECTION: FLANGE; BODY MATERIAL: A216 GR WCB; TRIM: A182F6; GRADE: A216 GR WCB; SOFTGOODS: PACKING GRAPHITE; STEM DESIGN: A182F6; APPLICATION: RUNNER SEAL ISOLATION; SPECIFICATION: CL 600; TYPE: ISOLATING; DESIGN RATING: ASME B19.34; TEMPERATURE RATING: ASME B16.34; CONNECTION ASME B16.5/B16.25; TESTING AND INSPECTION; API 598","Flowserve","GLOBE; ISOLATING","2 IN","A216 GR WCB","ASME B19.34; 102 BAR","A182F6","FLANGE","292.1 MM","N/S","HANDWHEEL, MANUAL","RUNNER SEAL ISOLATION","ASME B16.34; -29 TO 38 DEG C",null,null,"PACKING GRAPHITE"]
["Drakensberg Pumped Storage Scheme",640479,"VALVE, BUTTERFLY: TYPE: DRAIN WAFER; VALVE SIZE: DN 32; DESIGN RATING: PN25; TEMPERATURE RATING: NBR -10 TO 90 DEG C; CONNECTION: FLANGE; BODY MATERIAL: 2EN-GJS-4000-15(GGG-40) EPOXY COATED 120 UM; FACE TO FACE LENGTH: 33 MM; OPERATED: ACTUATOR PNEUMATIC; TRIM: A1.4408 INVESTMENT CASTING; SOFTGOODS: NBR; APPLICATION: SHAFT/RUNNER SEAL DRAIN; GRADE: DN 25-600; SPECIFICATION: D480; SCHEDULE: ASME B16.47; SERIES A; CL 150; SPECIAL FEATURES: BARE SHAFT; SUPPL P/N: D480 32W332A1NLF07 D11; CONNECTION TYPE; 3EN1092 PN16, OPERATING PRESSUE; 3.16 BAR, SHAFT MATERIAL; 1AISI420/1.4021, SHAFT LENGTH; 18, 18 MM, SEAT LINER; N NBR","KSB","BUTTERFLY; DRAIN WAFER","DN 32","2EN-GJS-4000-15(GGG-40) EPOXY COATED 120 UM","PN25","A1.4408 INVESTMENT CASTING","FLANGE","33 MM","N/S","ACTUATOR PNEUMATIC","SHAFT/RUNNER SEAL DRAIN","NBR -10 TO 90 DEG C","D480 32W332A1NLF07 D11",null,"NBR; R"]
["Drakensberg Pumped Storage Scheme",777978,"VALVE, SOLENOID: PIPE SIZE: 10 MM; STYLE: 4 PIPE CONNECTION 2 SOLENOID; POTENTIAL: 24 VDC; DESIGN RATING: 16 BAR; CONNECTION: 10 MM; BODY MATERIAL: ALUMININIUM; OPERATED: 24 V DC; ENCLOSURE RATING: 16 BAR; MEDIUM: AIR PNEUMATIC; OEM P/N: MPZWIDC.124 (0065745.002); PNEUMATIC CONTROL BLOCK, TYPE:MPZWIDC.124, ON WALL OR IN CABINET MOUNT, 2.5 KG, TWO CONTROL SOLENOIDS","Festo","SOLENOID; MPZWIDC.124, ON WALL OR IN CABINET MOUNT, 2.5 KG, TWO CONTROL SOLENOIDS","10 MM","ALUMINIUM","16 BAR","Stainless steel spool and armature with NBR (Buna-N) seals.","10 MM","95 mm","N/S","24 V DC","AIR PNEUMATIC","5°C to 39 deg","MPZWIDC.124 (0065745.002)","24 VDC; 16 BAR"]
["Drakensberg Pumped Storage Scheme",654743,"VALVE, BALL: VALVE SIZE: 1/2 IN; APPLICATION: AMMONIA SOLUTION LINE TO FEEDWATER TANK; TYPE: QUICK STOP; SUPPL P/N: N300","Spirax Sarco","BALL; QUICK STOP","1/2 IN","STEEL","N/S","N/S","TBC","N/S","N/S","Manual shut-off service","AMMONIA SOLUTION LINE TO FEEDWATER TANK","20–60 °C","N300"]
["Drakensberg Pumped Storage Scheme",662552,"VALVE, CHECK: TYPE: NON RETURN; VALVE SIZE: 80 MM; DESIGN RATING: PN40; TEMPERATURE RATING: 50 DEG C; CONNECTION: BW; BODY MATERIAL: CI; FACE TO FACE LENGTH: 173 MM; OPERATED: AUTOMATIC; TRIM: STL; APPLICATION: LIMESTONE HYDRAULIC FEEDER DRIVE; SPECIFICATION: TH-CD-2572-00-02; SUPPL P/N: 2572-00-02-14","KSB","CHECK; NON RETURN","80 MM","CI","PN40","STL","BW","173 MM","N/S","AUTOMATIC","LIMESTONE HYDRAULIC FEEDER DRIVE","50 DEG C","2572-00-02-14"]
["Drakensberg Pumped Storage Scheme",662572,"VALVE, CHECK: TYPE: NON RETURN; VALVE SIZE: 100 MM; DESIGN RATING: PN25; TEMPERATURE RATING: 55 DEG C; CONNECTION: BW; BODY MATERIAL: CAST STL; FACE TO FACE LENGTH: 170 MM; OPERATED: FLOW; TRIM: STL; APPLICATION: LIMESTONE HYDRAULIC FEEDER DRIVE; SPECIFICATION: TH-CD-2572-00-02; SUPPL P/N: 2572-00-02-25","KSB","CHECK; NON RETURN","100 MM","CAST STL","PN25","STL","BW","170 MM","N/S","FLOW","LIMESTONE HYDRAULIC FEEDER DRIVE","55 DEG C","2572-00-02-25"]
["Drakensberg Pumped Storage Scheme",696638,"VALVE, BUTTERFLY: TYPE: CENTERED DISC; VALVE SIZE: 3 IN; DESIGN RATING: PN35; TEMPERATURE RATING: 0-100 DEG C; CONNECTION: BW; BODY MATERIAL: 1.4571; FACE TO FACE LENGTH: 400 MM; OPERATED: MANUAL; TRIM: STL; SOFTGOODS: GASKETS; APPLICATION: DRAIN VALVE 1 TURBINE HOUSE UNIT 4; 4 0LCE10 AA401; SPECIFICATION: AV-25-63-SE-HR-G-XX-00; SUPPL P/N: 63906F3C7C3F09C3E0401EAC37FA0A05","KSB","BUTTERFLY; CENTERED DISC","3 IN",1.4571,"PN35","STL","BW","400 MM","N/S","MANUAL","DRAIN VALVE 1 TURBINE HOUSE UNIT 4","0-100 DEG C","63906F3C7C3F09C3E0401EAC37FA0A05",null,"GASKETS"]
["Drakensberg Pumped Storage Scheme",738822,"VALVE: TYPE: INJECTION; VALVE SIZE: 6/4 - R 1/2 IN; DESIGN RATING: 7-16 BAR; TEMPERATURE RATING: 25-40 DEG; CONNECTION: 6 MM COMPRESSION; OPERATED: STANDARD; BODY MATERIAL: PVC; .","Injection Valve / Dosing Valve","INJECTION","6/4 - R 1/2 IN","PVC","7-16 BAR","N/S","6 MM COMPRESSION","INJECTION; VALVE SIZE: 6/4 - R 104 s, Face-to-Face, Drilling / PCD, Mediums, Face-to-Face, Drilling / PCD, Medium","N/S","STANDARD","Chemical dosing / injection service","25-40 DEG"]
["Drakensberg Pumped Storage Scheme",738824,"VALVE: TYPE: FOOT; VALVE SIZE: 20 MM; DESIGN RATING: 7-16 BAR; TEMPERATURE RATING: 40 DEG; CONNECTION: 6 MM COMPRESSION; OPERATED: STANDARD; BODY MATERIAL: PVDF PTFE","Serto","FOOT","20 MM","PVDF PTFE","7-16 BAR","N/S","6 MM COMPRESSION","FOOT; VALVE SIZE: 2001 s, Face-to-Face, Drilling / PCD, Mediums, Face-to-Face, Drilling / PCD, Medium","N/S","STANDARD","Chemical dosing / suction foot valve service","40 DEG"]
["Drakensberg Pumped Storage Scheme",754488,"VALVE, SOLENOID: PIPE SIZE: G1/2 Thread ACRE; STYLE: 2/2-WAYS, NORMALLY CLOSED; POTENTIAL: 24 VDC; DESIGN RATING: PN 80 BAR; CONNECTION: GM84 - G1/2 THREADED PORT; BODY MATERIAL: MS BRASS; OPERATED: VOLTAGE; ENCLOSURE RATING: IP65; MEDIUM: WATER. AIR AND HYDRAULIC FLUIDS; POWER: 24 VDC; SUPPL P/N: 5404-A12,0EFMSGM84-C024/DC-12; BURKERT: 2/2-WAY-SOLENOID VALVE; SERVO-POSITION, 5404-A12,0EFMSGM84-C024/DC-12 A 2/2-WAYS;NORMALY CLOSED, ORIFICE SIZE - EF PTFE-SEAT-SEALING + FKM, MATERIAL - MS BRASS, PORT CONNECTION - GM84 G1/2 THREADED PORT, COIL SIZE - C 40 X 40, VOLTAGE - 024 24VOLTS, FREQUENCY - DC, POWER CONSUMPTION - 12 WATT, SPECIAL FEATURE MX13 PN 80 BAR RATED","Burkert","SOLENOID","G1/2 Thread ACRE","MS BRASS","PN 80 BAR","Stainless steel internals with PTFE seat and FKM (Viton) seal.","GM84 - G1/2 THREADED PORT; GM84 G1/2 THREADED PORT","95 acre","N/S","VOLTAGE","WATER. AIR AND HYDRAULIC FLUIDS","up to 200 deg","5404-A12,0EFMSGM84-C024/DC-12","24 VDC; IP65","D"]
["Drakensberg Pumped Storage Scheme",42716,"BODY: TYPE: PILOT VALVE; DIMENSIONS: DIA 15.5 X LG 36.4 MM; MATERIAL: BRASS; MODEL NO: 41; REFERENCE NO: 3W63625 T30; COMP; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Parker Hannifin","PILOT VALVE","36.4 MM","BRASS","150-600 Psi","Stainless steel internals with NBR/PTFE seat and stainless steel spring.","TBC","A2 x lg 36.4 mm","N/S","PRESSURE","Pilot Valve","up to 200 deg","3W63625 T30; 41"]
["Drakensberg Pumped Storage Scheme",41833,"VALVE: TYPE: COMPRESSOR; VALVE SIZE: 175 MM; OPERATED: PRESSURE; BODY MATERIAL: STL; TRIM: DISC SS; 2ND STAGE CONCENTRIC","Burckhardt Compression","COMPRESSOR","175 MM","STL","150-600 Psi","DISC SS","TBC","95 mm","N/S","PRESSURE","Compressor","40-80 deg"]
["Drakensberg Pumped Storage Scheme",41913,"ASSEMBLY: TYPE: PILOT VALVE; SUPPL P/N: R53608T10; REFERENCE NO: 10-11; COMPLETE; FOR DIESEL GENERATOR AIR STATOR COMPRESSOR; INGERSOLL RAND TYPE 30 MODEL 41","INGERSOLL RAND TYPE 30; Ingersoll Rand","PILOT VALVE","N/S","STMBLY:","10 BAR","N/S","TBC","70 mm","N/S","PRESSURE","Pilot Valve","20-80 deg","R53608T10; 10-11"]
["Drakensberg Pumped Storage Scheme",43215,"VALVE: VALVE SIZE: 68 MM; CONNECTION: COMPRESSION; OPERATED: PRESSURE; BODY MATERIAL: STL; TRIM: DISC STL; SUPPL P/N: 22K1R; REFERENCE NO: 30220479; COMPLETE; FOR TYPE 30 MODEL 41 ING-RAND AIR COMPRESSOR; SIZE 25.5MM THK","FOR TYPE 30; Ing-Rand","Compressor valve","68 MM","STL","N/A","DISC STL","COMPRESSION","3Ponnection: compression; operated: pressure; body material: stl; trim: disc stl","N/S","PRESSURE","AIR/OIL/WATER;","TBC","22K1R; 30220479"]
["Drakensberg Pumped Storage Scheme",43216,"VALVE: TYPE: DISCHARGE; VALVE SIZE: 68 MM; CONNECTION: COMPRESSION; OPERATED: PRESSURE; BODY MATERIAL: STL; TRIM: DISC STL; SUPPL P/N: CPN 30217947; REFERENCE NO: 30217947; 22K2R; SIZE 26.4MM THK; COMPLETE; FOR TYPE 30 MODEL 41 ING- RAND AIR COMPRESSOR","FOR TYPE 30","DISCHARGE","68 MM","STL","N/A","DISC STL","COMPRESSION","ENCE NO: 30217947; 22ENCE NO: 30217947; 22 ing / PCD, Mediuming / PCD, Medium","N/S","PRESSURE","AIR/OIL/WATER;","TBC","CPN 30217947; 30217947"]
["Drakensberg Pumped Storage Scheme",43234,"KIT, COMPRESSOR REPAIR: TYPE: TUNE UP/RING/VALVE; MODEL NO: 15T2; REFERENCE NO: 32226342; 32133951; FOR TYPE 30 COMPRESSOR","Ingersoll Rand","TUNE UP/RING/VALVE","Not specified","Not specified","N/A","Cast iron piston rings, stainless steel valve plates, hardened steel seats, spring steel springs, NBR/PTFE seals and fiber gaskets.","COMPRESSION","R3 ring/valve; model no: 15t2","N/S","PRESSURE","N/A","N/A","32226342; 15T2"]
["Drakensberg Pumped Storage Scheme",43262,"VALVE: TYPE: SUCTION; VALVE SIZE: 144 MM; CONNECTION: COMPRESSION; OPERATED: PRESSURE; BODY MATERIAL: STAINLESS STEEL; TRIM: DISC STL; REFERENCE NO: HT303811; 2ND STAGE; 20P-4PORTS; 46.3MM THK PLATE; 88MM THK O/A; WITH HEX NUT, WASHER AND SPLIT PIN","Burckhardt Compression","SUCTION","144 MM","STAINLESS STEEL","150-600 Psi","DISC STL","COMPRESSION","3T size: 144 mm; connection: compression; operated: pressure; body material: stainless steel; trim: disc stl; reference no: ht303811","N/S","PRESSURE","AIR/OIL/WATER;","−196 to +538 deg","HT303811"]
["Drakensberg Pumped Storage Scheme",43263,"VALVE: TYPE: SUCTION; VALVE SIZE: 104 MM; CONNECTION: COMPRESSION; OPERATED: PRESSURE; BODY MATERIAL: STL; STYLE: 2 PORT; TRIM: DISC STL; REFERENCE NO: HT303813; ASSY; 3RD STAGE 20P-2PORTS; 104MM DIA; 44.3MM THK PLATE; 88MM THK O/A; WITH HEX NUT; WASHER AND SPLIT PIN","Burckhardt Compression","SUCTION","104 MM","STL","N/A","DISC STL","COMPRESSION","95 mm","N/S","PRESSURE","AIR/OIL/WATER;","up to 100 deg","HT303813"]
["Drakensberg Pumped Storage Scheme",42019,"VALVE: VALVE SIZE: 10 MM; CONNECTION: COMPRESSION; OPERATED: PRESSURE; BODY MATERIAL: STL; STYLE: 5 WAY; TRIM: BONNET STL; REFERENCE NO: TC2G0340; THROTTLE AND CHECK MODULE","Hoerbiger","CHECK","10 MM","STL","N/A","BONNET STL","COMPRESSION","2Nonnection: compression; operated: pressure","N/S","PRESSURE","AIR/OIL/WATER;","up to 425 deg","TC2G0340"]
["Drakensberg Pumped Storage Scheme",42712,"CAP: TYPE: VALVE CAGE; DIMENSIONS: DIA 39 X HT 22 MM; MATERIAL: STL; REFERENCE NO: 3W75338; FOR 8K AIR HEAD ASSEMBLY; TYPE 30 MODEL 41 ING- RAND AIR COMPRESSOR","TYPE 30","VALVE CAGE","39 MM","STL","N/A","Steel valve cage with spring stainless steel valve plate, hardened steel seat, and spring steel spring assembly.","COMPRESSION","22 mm","N/S","PRESSURE","AIR/OIL/WATER;","up to 200 deg","3W75338"]
["Drakensberg Pumped Storage Scheme",43264,"VALVE: TYPE: SUCTION; VALVE SIZE: 104 MM; CONNECTION: COMPRESSION; OPERATED: PRESSURE; BODY MATERIAL: STAINLESS STEEL; TRIM: DISC STL; REFERENCE NO: HT303815; 4TH STAGE; 20P-2PORTS; 46.3MM THK PLATE; 89MM THK O/A; WITH HEX NUT, WASHER AND SPLIT PIN","Burckhardt Compression","SUCTION","104 MM","STAINLESS STEEL","N/A","DISC STL","COMPRESSION","3T size: 104 mm; connection: compression; operated: pressure; body material: stainless steel; trim: disc stl; reference no: ht303815","N/S","PRESSURE","AIR/OIL/WATER;","up to 120 deg","HT303815"]
["Drakensberg Pumped Storage Scheme",43265,"VALVE: TYPE: DISCHARGE; VALVE SIZE: 164 MM; CONNECTION: COMPRESSION; OPERATED: PRESSURE; BODY MATERIAL: STAINLESS STEEL; TRIM: DISC STL; REFERENCE NO: HT303810; ASSY; 1ST STAGE 20P- 5PORTS; 46.0MM THK PLATE; 70MM THK O/A; WITH HEX NUT AND SPLIT PIN","Burckhardt Compression","DISCHARGE","164 MM","STAINLESS STEEL","N/A","DISC STL","COMPRESSION","3 ve size: 164 mm; connection: compression; operated: pressure; body material: stainless steel; trim: disc stl; reference no: ht303810","N/S","PRESSURE","AIR/OIL/WATER;","80-120 deg","HT303810"]
["Drakensberg Pumped Storage Scheme",43268,"VALVE: TYPE: DISCHARGE; REFERENCE NO: HT303799; 34-00; 2ND STAGE; RETAINER ASSY","Burckhardt Compression","DISCHARGE","N/S","STEYP","N/A","Steel retainer with stainless steel valve plate, hardened steel seat and stop plate, spring steel springs.","COMPRESSION","N/S","N/S","PRESSURE","AIR/OIL/WATER;","100-160 deg","HT303799"]
["Drakensberg Pumped Storage Scheme",43269,"VALVE: TYPE: SUCTION; DRAWING NO: HT 303857 REV 1; REFERENCE NO: 35-00; 3RD STAGE; RETAINER ASSY","Burckhardt Compression","SUCTION","N/S","STEYP","N/A","Steel retainer assembly with stainless steel suction valve plate, hardened steel seat and stop plate, spring steel springs.","COMPRESSION","N/S","N/S","PRESSURE","AIR/OIL/WATER;","40-80 deg","35-00; HT 303857 REV 1"]
["Drakensberg Pumped Storage Scheme",43270,"VALVE: TYPE: DISCHARGE; REFERENCE NO: HT303800; 36-00; 3RD STAGE; RETAINER ASSY","Burckhardt Compression","DISCHARGE","N/S","STEYP","N/A","Steel retainer assembly with stainless steel discharge valve plate, hardened steel seat and stop plate, spring steel springs.","COMPRESSION","N/S","N/S","PRESSURE","AIR/OIL/WATER;","up to 150","HT303800"]
["Drakensberg Pumped Storage Scheme",43271,"VALVE: TYPE: SUCTION; REFERENCE NO: 37-00; HT303858; 4TH STAGE; RETAINER ASSY","Burckhardt Compression","SUCTION","N/S","STEYP","N/A","Steel retainer assembly with stainless steel suction valve plate, hardened steel seat and stop plate, spring steel springs.","COMPRESSION","N/S","N/S","PRESSURE","AIR/OIL/WATER;","up to 120 deg","37-00"]
["Drakensberg Pumped Storage Scheme",62413,"VALVE, SOLENOID: PIPE SIZE: 12 MM; STYLE: 4 WAY; POTENTIAL: 240 - 250 VDC; DESIGN RATING: 70-700 KPA; CONNECTION: FNPT; BODY MATERIAL: BRASS; OPERATED: PRESSURE; ENCLOSURE RATING: IP65 EN 60529; MEDIUM: AIR/OIL/WATER; POWER: 11.2 W; APPLICATION: BLOWDOWN COMPRESSOR; REFERENCE NO: WP8345E001; GENERAL PURPOSE ENCLOSURE; 240 VDC COIL","ASCO Numatics","SOLENOID","12 MM","BRASS","70-700 KPA","SS spool & armature with NBR seals and PTFE guide rings","FNPT","95 mm","N/S","PRESSURE","AIR/OIL/WATER; BLOWDOWN COMPRESSOR","80 deg","WP8345E001","240 - 250 VDC; 11.2 W; IP65 EN 60529"]
["Drakensberg Pumped Storage Scheme",44480,"CONTROL: TYPE: PUMP VALVE ASSY","Burckhardt Compression/Ingersoll Rand/KSB","PUMP VALVE ASSY","N/S","Not specified","N/A","Hardened steel spool/poppet with hardened seat, spring steel spring, and NBR/PTFE sealing system.","TBC","N/S","N/S","TBC","TBC","TBC"]
["Drakensberg Pumped Storage Scheme",61543,"ADAPTOR: TYPE: PILOT VALVE; MATERIAL: BRASS; REFERENCE NO: 3W39895; FOR TYPE 30 MODEL 15T2 ING-RAND AIR COMPRESSOR; SIZE 20MM DIA X 60MM LG","FOR TYPE 30; Ing-Rand","PILOT VALVE","20 MM","BRASS","N/A","Brass body with NBR seals and PTFE guide/seal elements","pilot valve assembly",";1 reference","N/S","pilot valve assembly","AIR","up to 200 deg","3W39895"]
["Drakensberg Pumped Storage Scheme",62540,"VALVE, SOLENOID: POTENTIAL: 220 V; SUPPL P/N: S2155","ASCO Numatics/Parker Hannifin/Festo","SOLENOID","N/S","STEOL","N/A","Stainless steel plunger and core with NBR seals and brass/stainless seat.","TBC","N/S","N/S","Electrically actuated valve","GAS/LIQUID","TBC","S2155","220 V"]
["Drakensberg Pumped Storage Scheme",62568,"VALVE, SOLENOID: PIPE SIZE: 10 MM; STYLE: 2 WAY; POTENTIAL: 220 VDC; DESIGN RATING: 100 BAR; CONNECTION: FNPT; BODY MATERIAL: BRASS; OPERATED: NC; ENCLOSURE RATING: IP65; MEDIUM: GAS/LIQUID; POWER: 16 W; REFERENCE NO: 9107500/0701","Burkert","SOLENOID","10 MM","BRASS","100 BAR","Stainless steel plunger and core with PTFE guide rings, FKM/NBR seals, and brass/stainless seat system.","FNPT","5OTENTIAL: 220 VDC; DESIGN RATING: 100 llinglling","N/S","NC","GAS/LIQUID","up to 200 deg","9107500/0701","220 VDC; 16 W; IP65"]
["Drakensberg Pumped Storage Scheme",63087,"VALVE, SOLENOID: PIPE SIZE: 10 MM; STYLE: 5 WAY; BODY MATERIAL: STEEL; OPERATED: DOUBLE ACTING; MEDIUM: LIQUID; YUKEN; ENCLOSURE: GENERAL PURPOSE; CONNECTION MANIFOLD","Yuken Kogyo","SOLENOID","10 MM","STEEL","N/A","Stainless steel plunger and core with PTFE guide rings, FKM/NBR seals, and hardened brass/stainless seat system.","Manifold mounted","95 mm","N/S","DOUBLE ACTING","LIQUID","−29 to +425 deg"]
["Drakensberg Pumped Storage Scheme",63152,"VALVE, GATE: VALVE SIZE: 3/4 IN; TYPE: SOLID WEDGE; CONNECTION: FLANGE; BODY MATERIAL: BRASS; TRIM: DISC BRS; OPERATED: HANDWHEEL; STEM DESIGN: INSIDE SCREW; STYLE: THD BONNET; NEEDLE VALVE; FLANGE SIZE 105MM O/D; 4 HOLES 14MM DIA PCD 75MM; BS 2060","Bristol Valves","GATE; SOLID WEDGE","3/4 IN","BRASS","N/A","DISC BRS; INSIDE SCREW","FLANGE","5; mm","75MM; 4 HOLES 14MM DIA PCD 75MM","HANDWHEEL","AIR/OIL/WATER;","up to 200 deg"]
["Drakensberg Pumped Storage Scheme",65785,"VALVE: TYPE: IMPULSE; VALVE SIZE: 15 MM; CONNECTION: THD FEMALE; OPERATED: PRESSURE; BODY MATERIAL: STL; TRIM: DISC STL; DRAWING NO: MB9-642.6350B REV 1; MANIFOLD; SIZE 18MM THK","Burckhardt Compression","IMPULSE","15 MM","STL","N/A","DISC STL","THD FEMALE","5S size: 15 mm; connection: thd female; operated: pressure","N/S","PRESSURE","TBC","TBC","MB9-642.6350B REV 1"]
["Drakensberg Pumped Storage Scheme",65786,"VALVE, GATE: VALVE SIZE: 250 MM; TYPE: SPHERICAL MANUAL BYPASS; CONNECTION: FLANGE; FACE TO FACE LENGTH: 250 MM; BODY MATERIAL: STEEL; OPERATED: HANDWHEEL; TEMPERATURE RATING: 16 DEG C; DESIGN RATING: 7.2 MPA; MAIN BY-PASS VALVE VOEST-ALPINE TYPE MB9-642-5320A ESKOM NO. 0.48/1121 DESIGNE PRESSURE = 7.2 MPA VALVE, BYPASS MAIN 5320 A","MB9-642-5320A","GATE; BYPASS MAIN 5320 A; SPHERICAL MANUAL BYPASS","250 MM","STEEL","7.2 MPA","13Cr/Alloy steel spherical wedge, Stellite hard-faced seats, SS stem, graphite packing","FLANGE","250 MM","N/S","HANDWHEEL","WATER","16 DEG C"]
["Drakensberg Pumped Storage Scheme",63285,"VALVE, RELIEF: VALVE SIZE: 12 MM; CONNECTION: FNPT; BODY MATERIAL: STL; TRIM: SPRING STL; OPERATED: PRESSURE; REFERENCE NO: M67E; HP UNIT PILOT; DAIKIN","Daikin Industries","RELIEF","12 MM","STL","N/A","SPRING STL","FNPT","3E12 mm","N/S","PRESSURE","AIR,WATER,OIL","−29 to +425 deg","M67E"]
["Drakensberg Pumped Storage Scheme",63348,"VALVE, BALL: VALVE SIZE: 3/4 IN; DESIGN RATING: 1000 KPA; CONNECTION: FEMALE THD; OPERATED: LEVER; STYLE: 3 WAY; 3 PIECE; TRIM: BALL SS GR 316; SOFTGOODS: SEALS PTFE; GRADE: CF8M; ACID WATER OIL AND GAS; THROUGHWAY IN BALL TO BE 20 MM","Parker Hannifin","BALL","3/4 IN","MEEAL","1000 KPA","BALL SS GR 316","FEMALE THD","334 in","N/S","LEVER","Acid Water, Oil and Gas","5-100 deg",null,null,"SEALS PTFE"]
["Drakensberg Pumped Storage Scheme",63385,"SEAT: TYPE: DISC SAFETY VALVE; DIMENSIONS: SQ 0.514 IN; MATERIAL: 1.4122 DIN X 35CRMO17; SUPPL P/N: 018109610; 601267620; MODEL NO: VSE2.40.25.A.50.I.22.123; USED ON SEMPELL; POSITION CODE RL01S010, RL02S009, RL03S008","Sempell","DISC SAFETY VALVE","13.06MM","1.4122 DIN X 35CRMO17","N/A","1.4122 stainless steel seat with hardened/stainless disc interface","TBC","N/S","N/S","TBC","SEMPELL","up to 450","018109610; VSE2.40.25.A.50.I.22.123",null,"TYPE: DISC SAFETY VALVE"]
["Drakensberg Pumped Storage Scheme",63532,"VALVE, GATE: VALVE SIZE: 32 MM; TYPE: WEDGE; CONNECTION: THD; BODY MATERIAL: BRASS; TRIM: DISC/STEM BRS; OPERATED: HANDWHEEL; STEM DESIGN: NON RISING; STYLE: THD BONNET; TEMPERATURE RATING: 175 DEG C; DESIGN RATING: 1600 KPA; REFERENCE NO: 1001-125; SUPPLIER NOTE: TO BE SUPPLIED ACCORDING TO S.A.B.S. SPECIFICATION WITH A PRESSURE CERTIFICATE; CLASS 125","Pegler Yorkshire","GATE; WEDGE","32 MM","BRASS","1600 KPA","DISC/STEM BRS; NON RISING","THD","N/S","N/S","HANDWHEEL","AIR,WATER,OIL","175 DEG C","1001-125",null,null,"CERTIFICATE"]
["Drakensberg Pumped Storage Scheme",65784,"VALVE: TYPE: MAIN CONTROL; VALVE SIZE: 100 MM; OPERATED: PRESSURE; BODY MATERIAL: STL; STYLE: 2 WAY; TRIM: BONNET STL; REFERENCE NO: MB9-642.6300C; CONNECTION MANIFOLD","Burckhardt Compression","MAIN CONTROL","100 MM","STL","N/A","BONNET STL","Manifold mounted","N/S","N/S","PRESSURE","Main Control","N/S","MB9-642.6300C"]
["Drakensberg Pumped Storage Scheme",65929,"VALVE, RELIEF: VALVE SIZE: 25 MM; SET PRESSURE: 1015 LB; CONNECTION: FNPT; BODY MATERIAL: CI; TRIM: DISC SS; SPRING STL; OPERATED: PRESSURE, SPRING; REFERENCE NO: 83C88-81; SAFETY; SERIES 80 SRV","Consolidated / Baker Hughes","RELIEF","25 MM","CI","1015 LB","DISC SS","FNPT","N/S","N/S","PRESSURE, SPRING","Safety / Pressure Relief","180 deg","83C88-81"]
["Drakensberg Pumped Storage Scheme",66050,"VALVE, GATE: VALVE SIZE: 1-1/2 IN; TYPE: SOLID WEDGE; CONNECTION: FNPT; BODY MATERIAL: BRASS; TRIM: DISC BRS; OPERATED: HANDWHEEL; STEM DESIGN: INSIDE SCREW; STYLE: THD BONNET; DESIGN RATING: 2000 KPA; COBRA","Cobra Watertech","GATE; SOLID WEDGE","1-1/2 IN","BRASS","2000 KPA","DISC BRS; INSIDE SCREW","FNPT","N/S","N/S","HANDWHEEL","water, hot water, and general fluid","5-80 deg"]
["Drakensberg Pumped Storage Scheme",65807,"VALVE: TYPE: FLOW CONTROL; VALVE SIZE: 15 MM; CONNECTION: FNPT; OPERATED: PRESSURE; BODY MATERIAL: STL; STYLE: 2 WAY; TRIM: BONNET STL; REFERENCE NO: PCM-600; FOR HIGH PRESSURE OIL FLOW; COLORFLOW","Colorflow","FLOW CONTROL","15 MM","STL","N/A","BONNET STL","FNPT","5Wvalve size: 15 mm; connection: fnpt; operated: pressure; body material: stl","N/S","PRESSURE","Flow Control (High Pressure Oil Flow)","−29 to +425 deg","PCM-600"]
["Drakensberg Pumped Storage Scheme",65808,"VALVE, GLOBE: VALVE SIZE: 3/4 IN; OPERATED: HANDWHEEL; CONNECTION: FLANGE; BODY MATERIAL: STL; TRIM: BONNET STL; STEM DESIGN: INSIDE SCREW; STYLE: BOLTED BONNET; REFERENCE NO: Y237A-4","Yarway","GLOBE","3/4 IN","STL","N/S","BONNET STL; INSIDE SCREW","FLANGE","5S/4 in","N/S","HANDWHEEL","liquid, steam, gas","40 to 120 deg","Y237A-4"]
["Drakensberg Pumped Storage Scheme",66072,"VALVE, CHECK: TYPE: PISTON; VALVE SIZE: 25 MM; CONNECTION: NPT; BODY MATERIAL: STAINLESS STEEL; STYLE: THD CAP; TRIM: DISC/CAP STL; NON-RETURN; EO; TUBE SIZE 25MM OD EO TUBE CONNECTION AT BOTH ENDS","Parker Hannifin","CHECK; PISTON","25 MM","STAINLESS STEEL","N/S","DISC/CAP STL","NPT","190 mm","N/S","Hydraulic/tube system service","oil, hydraulic fluid, gas","−196 to +538 deg"]
["Drakensberg Pumped Storage Scheme",65832,"VALVE: TYPE: ISOLATING; VALVE SIZE: 65 MM; CONNECTION: THD; OPERATED: HANDWHEEL; BODY MATERIAL: STL; STYLE: THD BONNET; TRIM: DISC/STEM SS; PRESS TANK PUMP UNLOADER","Burckhardt Compression/Parker Hannifin/KSB","ISOLATING","65 MM","STL","N/S","DISC/STEM SS","THD","5Ove size: 65 mm; connection: thd","N/S","HANDWHEEL","pressure tank and pump unloader isolation","−29 to +425 deg"]
["Drakensberg Pumped Storage Scheme",65847,"VALVE, NEEDLE: VALVE SIZE: 60 MM; BODY MATERIAL: STL; FACE TO FACE LENGTH: 120 MM; REFERENCE NO: MB9-642-5362E; NOZZLE","Burckhardt Compression","NEEDLE","60 MM","STL","N/S","SS needle & stem with hardened nozzle seat and graphite packing","Nozzle connection","120 mm ","N/S","Flow regulation","precise flow control, throttling","up to 425 deg","MB9-642-5362E"]
["Drakensberg Pumped Storage Scheme",65861,"VALVE, PILOT: VALVE SIZE: 5 MM; MATERIAL: BRASS; REFERENCE NO: MB8-288-1705D; SIZE 6MM LG; CONNECTION COMPRESSION; STYLE 4 WAY; TRIM SS STEM; PRESSURE OPERATED; COMPLETE WITH PISTON; X5CRNI 189; GROUP 1700; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Burckhardt Compression","PILOT","5 MM","BRASS","N/S","SS piston & stem with brass seat and NBR/PTFE seals","COMPRESSION","95 mm","N/S","PRESSURE","Pilot / Control Service","up to 200 deg","MB8-288-1705D"]
["Drakensberg Pumped Storage Scheme",66073,"VALVE, RELIEF: VALVE SIZE: 12 MM; SET PRESSURE: 400 BAR; CONNECTION: FNPT; BODY MATERIAL: STL; TRIM: SPRING STL; OPERATED: PRESSURE, SPRING; REXROTH PRESSURE; HYDRONORMA","Rexroth","RELIEF","12 MM","STL","400 BAR","SPRING STL","FNPT","95 mm","N/S","PRESSURE, SPRING","AIR,WATER,OIL","−29 to +425 deg"]
["Drakensberg Pumped Storage Scheme",65917,"VALVE, RELIEF: VALVE SIZE: 45 X 40 MM; SET PRESSURE: 70 BAR; CONNECTION: NPT X FNPT; BODY MATERIAL: STL; TRIM: DISC/SPRING STL; OPERATED: PRESSURE, SPRING; SAFETY","Bopp & Reuther","RELIEF","45 X 40 MM","STL","70 BAR","DISC/SPRING STL","NPT X FNPT","N/S","N/S","PRESSURE, SPRING","AIR,WATER,OIL","up to 425 deg"]
["Drakensberg Pumped Storage Scheme",66074,"VALVE, BALL: VALVE SIZE: 16 MM; DESIGN RATING: 100 BAR; TEMPERATURE RATING: -200 TO 200 DEG C; CONNECTION: NPT X FNPT; BODY MATERIAL: STEEL; OPERATED: LEVER; STYLE: 4 WAY; TRIM: BALL STL; SPECIFICATION: DIN 3230; PORT TYPE: 3 X MALE; 1 X FEMALE; APPLICATION: UPSTREAM SEAL CHANGE OVER VALVE; TYPE: MANUAL OPERATED; SUPPL P/N: 1017489; REFERENCE NO: 1017489; 3 MALE X 1 FEMALE; CHANGE-OVER; BLOCK; ARGUS","Argus","BALL; 3 X MALE; MANUAL OPERATED","16 MM","STEEL","100 BAR","BALL STL","NPT X FNPT","95 mm","N/S","LEVER","UPSTREAM SEAL CHANGE OVER VALVE","-200 TO 200 DEG C",1017489]
["Drakensberg Pumped Storage Scheme",66234,"VALVE, DIAPHRAGM: VALVE SIZE: 32 MM; CONNECTION: FNPT; BODY MATERIAL: CI; DIAPHRAGM MATERIAL: RUBBER GR Q; OPERATED: HANDWHEEL; STYLE: WEIR; SAUNDERS; TYPE A","Saunders","DIAPHRAGM","32 MM","CI; RUBBER GR Q","N/S","RUBBER GR Q","FNPT","A6 fnpt","N/S","HANDWHEEL","Isolation / throttling of corrosive, abrasive, slurry, water, chemical, and process fluids","up to 90 deg"]
["Drakensberg Pumped Storage Scheme",66076,"VALVE, NEEDLE: VALVE SIZE: 3.5 MM; CONNECTION: THD MALE X FEMALE; BODY MATERIAL: BRASS; OPERATED: HANDWHEEL; TRIM: DISC STL; THD BONNET; BLOCKING VALVE; P.17","Parker Hannifin","NEEDLE","3.5 MM","BRASS","N/S","DISC STL","THD MALE X FEMALE","6:3.5 mm","N/S","HANDWHEEL","AIR/OIL/WATER;","up to 200 deg"]
["Drakensberg Pumped Storage Scheme",66235,"VALVE, DIAPHRAGM: VALVE SIZE: 40 MM; CONNECTION: FNPT; BODY MATERIAL: CI; DIAPHRAGM MATERIAL: RUBBER GR Q; OPERATED: HANDWHEEL; STYLE: WEIR; SAUNDERS; TYPE A","Saunders","DIAPHRAGM","40 MM","CI; RUBBER GR Q","N/S","RUBBER GR Q","FNPT","A6 fnpt","N/S","HANDWHEEL","Sewage and wastewater, Water,Process water","up to 90 deg"]
["Drakensberg Pumped Storage Scheme",66236,"VALVE, DIAPHRAGM: VALVE SIZE: 50 MM; CONNECTION: FNPT; BODY MATERIAL: CI; DIAPHRAGM MATERIAL: RUBBER GR Q; OPERATED: HANDWHEEL; STYLE: WEIR; SAUNDERS","Saunders","DIAPHRAGM","50 MM","CI; RUBBER GR Q","N/S","RUBBER GR Q","FNPT","A6 fnpt","N/S","HANDWHEEL","Sewage and wastewater, Water,Process water","up to 90 deg"]
["Drakensberg Pumped Storage Scheme",66205,"VALVE, RELIEF: SET PRESSURE: 60 BAR; REFERENCE NO: MB8-222-2450C60B; SAFETY","Burckhardt Compression","RELIEF","N/S","STEEL","60 BAR","SS disc & seat, SS spindle, chrome alloy spring (metal-seated safety valve)","TBC","N/S","N/S","PRESSURE","Safety Protection","180 deg","MB8-222-2450C60B"]
["Drakensberg Pumped Storage Scheme",66327,"VALVE: TYPE: COMPENSATION; VALVE SIZE: 16 MM; CONNECTION: SLIP ON; OPERATED: LEVER; BODY MATERIAL: STAINLESS STEEL; STYLE: 3 WAY; TRIM: BONNET SS; GPS","GPS Valve (probable)","COMPENSATION","16 MM","STAINLESS STEEL","N/S","BONNET SS","SLIP ON","6Lvalve size: 16 mm; connection: slip on","N/S","LEVER","Air,Gas,Liquid","−196 to +538 deg"]
["Drakensberg Pumped Storage Scheme",66223,"VALVE, SOLENOID: PIPE SIZE: 25 MM; STYLE: 4 WAY; POTENTIAL: 110/120 VAC; DESIGN RATING: 3000 LB; BODY MATERIAL: STEEL; MEDIUM: OIL; CURRENT: 0.72-0.75 A; MODEL NO: D63W1B1Y 34; 50/60 HZ; CONNECTION MANIFOLD; GENERAL PURPOSE ENCLOSURE; DIRECTIONAL CONTROL VALVE","Yuken Kogyo","SOLENOID","25 MM","STEEL","3000 LB","Hardened steel spool with SS armature and NBR/PTFE seals","Manifold mounted","190 mm","N/S","SOLENOID","OIL","−29 to +425 deg","D63W1B1Y 34","110/120 VAC; 0.72-0.75 A"]
["Drakensberg Pumped Storage Scheme",66232,"VALVE, DIAPHRAGM: VALVE SIZE: 15 MM; CONNECTION: FNPT; BODY MATERIAL: CI; DIAPHRAGM MATERIAL: RUBBER GR Q; OPERATED: HANDWHEEL; STYLE: WEIR; REFERENCE NO: A; SAUNDERS","Saunders","DIAPHRAGM","15 MM","CI; RUBBER GR Q","N/S","RUBBER GR Q","FNPT","A6 fnpt","N/S","HANDWHEEL","Water, slurry, or compatible process fluid","20-90 deg","A"]
["Drakensberg Pumped Storage Scheme",66233,"VALVE, DIAPHRAGM: VALVE SIZE: 25 MM; CONNECTION: FNPT; BODY MATERIAL: CI; DIAPHRAGM MATERIAL: RUBBER GR Q; OPERATED: HANDWHEEL; STYLE: WEIR; SAUNDERS; TYPE A","Saunders","DIAPHRAGM","25 MM","CI; RUBBER GR Q","N/S","RUBBER GR Q","FNPT","A6 fnpt","N/S","HANDWHEEL","Water / Slurry Service","20-90 deg"]
["Drakensberg Pumped Storage Scheme",66493,"VALVE, CHECK: TYPE: PISTON; VALVE SIZE: 12 MM; CONNECTION: NPT; BODY MATERIAL: STL; STYLE: THD CAP; TRIM: DISC STL; SUPPL P/N: RHD12-PL; NON-RETURN; EO; TUBE CONNECTION AT BOTH ENDS","Parker Hannifin","CHECK; PISTON","12 MM","STL","N/S","DISC STL","NPT","190 mm","N/S","PRESSURE","Hydraulic oil/Low-flammability hydraulic fluids","20-120 deg","RHD12-PL"]
["Drakensberg Pumped Storage Scheme",66494,"SPOOL: TYPE: RELIEF VALVE; INSIDE DIAMETER: 108 MM; LENGTH: 153 MM; MATERIAL: STL; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Burckhardt Compression","RELIEF VALVE","108 MM","STL","N/S","Hardened steel spool with PTFE guide rings and hardened sealing surfaces","TBC","95 mm","N/S","PRESSURE","hydraulic oil / hydraulic fluid service","up to 425 deg"]
["Drakensberg Pumped Storage Scheme",66522,"VALVE, GATE: VALVE SIZE: 400 MM; TYPE: SOLID WEDGE; CONNECTION: FLANGE; BODY MATERIAL: STL; TRIM: BONNET STL; OPERATED: HANDWHEEL; STEM DESIGN: RISING OUTSIDE SCREW; STYLE: BOLTED BONNET; CAST; HYDRO TEST CERTIFICATE REQUIRED","Flowserve","GATE; SOLID WEDGE","400 MM","STL","ANSI Class 150/300/600","BONNET STL; RISING OUTSIDE SCREW","FLANGE","6R0 mm","N/S","HANDWHEEL","Industrial process fluid service","up to 425 deg",{"$nulls":3},"CERTIFICATE REQUIRED"]
["Drakensberg Pumped Storage Scheme",66523,"VALVE, GATE: VALVE SIZE: 300 MM; TYPE: SOLID WEDGE; CONNECTION: FLANGE; BODY MATERIAL: STL CAST; TRIM: BONNET STL; OPERATED: HANDWHEEL, GEAR; STEM DESIGN: RISING OS; STYLE: BOLTED BONNET; DESIGN RATING: 100 BAR; HYDRO TEST CERTIFICATE REQUIRED; REFER TO CONTRACT OPY 49218","Velan","GATE; SOLID WEDGE","300 MM","STL CAST","100 BAR","BONNET STL; RISING OS","FLANGE","610 rilling / PCD, Mediumrilling / PCD, Medium","N/S","HANDWHEEL, GEAR","High-pressure industrial process service","up to 425 deg",{"$nulls":3},"CERTIFICATE REQUIRED"]
["Drakensberg Pumped Storage Scheme",66524,"VALVE, GATE: VALVE SIZE: 250 MM; TYPE: SOLID WEDGE; CONNECTION: FLANGE; BODY MATERIAL: CS; TRIM: BONNET STL; OPERATED: HANDWHEEL; STEM DESIGN: RISING OUTSIDE SCREW; STYLE: BOLTED BONNET","Flowserve","GATE; SOLID WEDGE","250 MM","CS","ANSI Class 150/300/600","BONNET STL; RISING OUTSIDE SCREW","FLANGE","6A0 mm","N/S","HANDWHEEL","High-pressure industrial process service","150 deg"]
["Drakensberg Pumped Storage Scheme",66525,"VALVE, GATE: VALVE SIZE: 200 MM; CONNECTION: FLANGE; BODY MATERIAL: STL CAST; TRIM: BONNET STL; OPERATED: HANDWHEEL; STEM DESIGN: RISING OS; STYLE: BOLTED BONNET","Flowserve","GATE","200 MM","STL CAST","ANSI Class 150/300/600","BONNET STL; RISING OS","FLANGE","6E0 mm","N/S","HANDWHEEL","High-pressure industrial process service","150 deg"]
["Drakensberg Pumped Storage Scheme",66530,"VALVE: VALVE SIZE: 250 MM; BODY MATERIAL: CS; FIG NO: 16SMZ; NON-RETURN; SIZE 10; HYDRO.TEST CERTIFICATE REQUIRED FOR ALL VALVES","Check-Rite Valves","Non-return valve / Check valve","250 MM","CS","N/S","SS disc, hard-faced seat, SS hinge, graphite/PTFE seals","TBC","E6 cs","N/S","PRESSURE","Process fluid service","150 deg","16SMZ",null,null,"CERTIFICATE REQUIRED FOR ALL VALVES"]
["Drakensberg Pumped Storage Scheme",66527,"VALVE, BUTTERFLY: TYPE: WAFER; VALVE SIZE: 400 MM; CONNECTION: FLANGE; BODY MATERIAL: CS; OPERATED: GEAR; TRIM: DISC STL RUBBERIZED; REFERENCE NO: 051100A492183; BOVING; COMPLETE WITH MASTERGEAR OPERATOR AND HANDWHEEL; HYDRO TEST CERTIFICATE REQUIRED FOR ALL VALVES","Boving","BUTTERFLY; WAFER","400 MM","CS","N/S","DISC STL RUBBERIZED","FLANGE","95 mm","N/S","GEAR","Industrial process fluid service","80 deg","051100A492183",null,null,"CERTIFICATE REQUIRED FOR ALL VALVES"]
["Drakensberg Pumped Storage Scheme",66531,"VALVE, CHECK: TYPE: SWING; VALVE SIZE: 80 MM; CONNECTION: COMPRESSION; BODY MATERIAL: CS; TRIM: DISC STL; FIG NO: 16SMZ; CHECKRITE NON-RETURN; HYDRO TEST CERTIFICATE REQUIRED FOR ALL VALVES","Check-Rite Valves","CHECK; SWING","80 MM","CS","N/S","DISC STL","COMPRESSION","190 mm","N/S","PRESSURE","Process fluid service","150 deg","16SMZ",null,null,"CERTIFICATE REQUIRED FOR ALL VALVES"]
["Drakensberg Pumped Storage Scheme",66529,"VALVE, CHECK: TYPE: SWING; VALVE SIZE: 400 MM; DESIGN RATING: 16 BAR; CONNECTION: FLANGE; BODY MATERIAL: CS; TRIM: BONNET/DISC STEEL; REFERENCE NO: 16SMZ; CHECKRITE NON-RETURN; HYDRO. TEST CERTIFICATE REQUIRED FOR ALL VALVES","Check-Rite Valves","CHECK; SWING","400 MM","CS","16 BAR","BONNET/DISC STEEL","FLANGE","6:valve size: 400 mm; design rating: 16 bar; connection: flange","N/S","PRESSURE","Process fluid service","150 deg","16SMZ",null,null,"CERTIFICATE REQUIRED FOR ALL VALVES"]
["Drakensberg Pumped Storage Scheme",69572,"VALVE, GATE: VALVE SIZE: 40 MM; CONNECTION: FLANGE; OPERATED: HANDWHEEL; FIG NO: H9-107; REFERENCE NO: W.P.9/1500; BONNEY FORGE","Bonney Forge","GATE","40 MM","STEAT","1500 PSI (WP) / Class 1500 Equivalent","(410 SS + Stellite hardfacing) for industrial pipeline gate valves","FLANGE","N/S","N/S","HANDWHEEL","Industrial/process service","250 deg","W.P.9/1500; H9-107"]
["Drakensberg Pumped Storage Scheme",66533,"VALVE, RELIEF: VALVE SIZE: 200 MM; BODY MATERIAL: STL CAST; OPERATED: PRESSURE; CAT NO: 50A-01B; CLAYTON","Cla-Val (Clayton)","RELIEF","200 MM","STL CAST","N/S","N/S","TBC","95 mm","N/S","PRESSURE","Pressure relief service for process systems","80 deg","50A-01B"]
["Drakensberg Pumped Storage Scheme",66534,"VALVE: TYPE: DELUGE; VALVE SIZE: 150 MM; DESIGN RATING: 150 LB; CONNECTION: FLANGE; OPERATED: AIR; BODY MATERIAL: BRASS; STYLE: 2 WAY; TRIM: BONNET BRS; SPECIFICATION: BS 4504; N.P. 16/3","Claval","DELUGE","150 MM","BRASS","150 LB","BONNET BRS","FLANGE","N/S","N/S","AIR","Fire protection / water deluge system service","50 deg"]
["Drakensberg Pumped Storage Scheme",66535,"VALVE, BALL: VALVE SIZE: 1/2 IN; DESIGN RATING: 40 LB; TEMPERATURE RATING: 25 DEG C; CONNECTION: FNPT; BODY MATERIAL: STAINLESS STEEL; OPERATED: LEVER; STYLE: UNION BONNET; TRIM: BALL SS; BRASS; WITH FIXED FEMALE FLANGE EITHER END","Swagelok","BALL","1/2 IN","STAINLESS STEEL","40 LB","BALL SS","FNPT","N/S","N/S","LEVER","General process/instrument service","25 DEG C"]
["Drakensberg Pumped Storage Scheme",66661,"VALVE, RELIEF: VALVE SIZE: 20 MM; BODY MATERIAL: STL; TRIM: BONNET/SPRING STL; OPERATED: PRESSURE; REFERENCE NO: 936-36275; L.P.; ABEX DENISON; MANIFOLD","Denison Hydraulics (formerly Abex-Denison)","RELIEF","20 MM","STL","N/S","BONNET/SPRING STL","TBC","N/S","N/S","PRESSURE","Hydraulic pressure relief service","80 deg","936-36275"]
["Drakensberg Pumped Storage Scheme",67279,"VALVE, BUTTERFLY: TYPE: WAFER; VALVE SIZE: 65 MM; DESIGN RATING: 16 BAR; CONNECTION: CLAMP; BODY MATERIAL: CI; OPERATED: LEVER; TRIM: DISC/SHAFT SS GR 316; SEAT EPDM; REFERENCE NO: 065-515-6S; DISC/SHAFT HEXAGON MACHINED CENTRE HOLE; LINER: E.P.D.M; SEAT TEST PRESSURE: 18 BAR; BODY TEST PRESSURE: 24 BAR; MATERIAL AND TEST CERTIFICATES TO DIN 50049/3.1B ARE TO BE SUPPLIED ON DELIVERY","Boehmer (probable)","BUTTERFLY; WAFER","65 MM","CI","16 BAR","DISC/SHAFT SS GR 316","CLAMP","95 mm","N/S","LEVER","Water/process fluid service","80 deg","065-515-6S",null,"M; 18 BAR","CERTIFICATES TO DIN 50049/3"]
["Drakensberg Pumped Storage Scheme",68148,"VALVE, RELIEF: VALVE SIZE: 50 MM; SET PRESSURE: 35 KPA; CONNECTION: THD; BODY MATERIAL: STL; TRIM: BRASS; OPERATED: SPRING; PRESSURE RANGE: 2-20 LB; REFERENCE NO: MD0014; SAFETY; TYPE 616-2; TYPE: HLP","Hale Hamilton","RELIEF; HLP","50 MM","STL","2-20 LB; 35 KPA","BRASS","THD","100 mm","N/S","SPRING","Pressure relief service","80 deg","MD0014"]
["Drakensberg Pumped Storage Scheme",68767,"VALVE: TYPE: CONTROL; VALVE SIZE: 12 MM; CONNECTION: FNPT; OPERATED: PRESSURE; BODY MATERIAL: STL; STYLE: 4 WAY; TRIM: DISC STL; REFERENCE NO: MB9-642-6500B; SIZE 15MM THK; FOR LOCKING VALVE 620/1","Burckhardt Compression","CONTROL","12 MM","STL","N/S","DISC STL","FNPT","N/S","N/S","PRESSURE","Control/locking valve service","80 deg","MB9-642-6500B"]
["Drakensberg Pumped Storage Scheme",68909,"ASSEMBLY: TYPE: BFPT DISCHARGE ISOLATOR VALVE BELT; SUPPL P/N: 324-39; FIG NO: M279400W; BRISCH CODE: L9571-501 HOPKINSONS VALVE, 100NB","Hopkinsons Valve","100NB; BFPT DISCHARGE ISOLATOR VALVE BELT","100 MM","Not specified","N/S","N/S","TBC","N/S","N/S","TBC","water system application","TBC","324-39; M279400W"]
["Drakensberg Pumped Storage Scheme",68910,"VALVE, GLOBE: VALVE SIZE: 1/2 IN; OPERATED: HANDWHEEL; CONNECTION: BW; BODY MATERIAL: CS ASTM A105; TRIM: DISC/SEAT HF; STEM SS GR 410; STEM DESIGN: RISING SPINDLE; STYLE: INTEGRAL BONNET; Y BODY; DESIGN RATING: 2500 PSI; TEMPERATURE RATING: 840 DEG F; REFERENCE NO: 578; VELAN","Velan","GLOBE","1/2 IN","CS ASTM A105","2500 PSI","DISC/SEAT HF; RISING SPINDLE","BW","N/S","N/S","HANDWHEEL","High-pressure process service","840 DEG F",578,null,"F"]
["Drakensberg Pumped Storage Scheme",72009,"VALVE, BALL: VALVE SIZE: 16 MM; DESIGN RATING: 400 LB; CONNECTION: FNPT; BODY MATERIAL: STEEL; OPERATED: LEVER; STYLE: 2 WAY; TRIM: BALL STL; SUPPL P/N: BH-B400-716; BOHMER; BLOCK","Bohmer","BALL","16 MM","STEEL","400 LB","BALL STL","FNPT","N/S","N/S","LEVER","High-pressure process fluid service","150 deg","BH-B400-716"]
["Drakensberg Pumped Storage Scheme",70478,"VALVE, RELIEF: VALVE SIZE: 50 X 32 MM; SET PRESSURE: 600 KPA; TEMPERATURE RATING: -10 TO 14 DEG C; CONNECTION: FLANGE; BODY MATERIAL: CI; TRIM: STAINLESS STEEL; OPERATED: PRESSURE; DESIGN RATING: 16 BAR; PRESSURE RANGE: 6 BAR; FIG NO: 4411/H2; REFERENCE NO: 16; SAFETY; INLET AND OUTLET PN16; TO SIZED TO DIN3320 AND TEST APPROVED IN ACCORDANCE WITH (AD-MERKBLATT A2); FLOW CAPACITY TO BE AT LEAST 35000 KG/HR","HEROSE","RELIEF","50 X 32 MM","CI","16 BAR; 6 BAR; 600 KPA","STAINLESS STEEL","FLANGE","95 mm","N/S","PRESSURE","Pressure relief service","-10 TO 14 DEG C","16; 4411/H2"]
["Drakensberg Pumped Storage Scheme",72010,"VALVE, BALL: VALVE SIZE: 20 MM; DESIGN RATING: 315; CONNECTION: FNPT; BODY MATERIAL: STEEL; OPERATED: LEVER; STYLE: 2 WAY; TRIM: BALL STL; BLOCK; BOHMER","Bohmer","BALL","20 MM","STEEL",315,"BALL STL","FNPT","95 mm","N/S","LEVER","Process fluid / hydraulic service","150 deg"]
["Drakensberg Pumped Storage Scheme",72012,"VALVE, BALL: VALVE SIZE: 50 MM; DESIGN RATING: 6 BAR; CONNECTION: FLANGE; BODY MATERIAL: STEEL; OPERATED: LEVER; STYLE: 2 WAY; TRIM: BALL STL; BOHMER; SERIES FK","Bohmer","BALL","50 MM","STEEL","6 BAR","BALL STL","FLANGE","95 mm","N/S","LEVER","Process fluid service","150 deg"]
["Drakensberg Pumped Storage Scheme",72002,"VALVE, BALL: VALVE SIZE: 50 MM; DESIGN RATING: 100 BAR; CONNECTION: FLANGE; BODY MATERIAL: STEEL; OPERATED: LEVER; STYLE: 2 WAY; TRIM: BALL STL; BOHMER","Bohmer","BALL","50 MM","STEEL","100 BAR","BALL STL","FLANGE","95 mm","N/S","LEVER","High-pressure process fluid service","150 deg"]
["Drakensberg Pumped Storage Scheme",72004,"VALVE, BALL: VALVE SIZE: 40 MM; DESIGN RATING: 100; CONNECTION: FNPT; BODY MATERIAL: STEEL; OPERATED: LEVER; STYLE: 2 WAY; TRIM: BALL STL; GRADE: C22.8; REFERENCE NO: 3101-0040-598166; SHUT-OFF; ARGUS","Argus","BALL","40 MM","STEEL",100,"BALL STL","FNPT","N/S","N/S","LEVER","Shut-off/isolation service","150 deg","3101-0040-598166"]
["Drakensberg Pumped Storage Scheme",72013,"VALVE, BALL: VALVE SIZE: 10 MM; DESIGN RATING: 500 LB; CONNECTION: FNPT; BODY MATERIAL: STEEL; OPERATED: LEVER; STYLE: 2 WAY; TRIM: BALL STL; SUPPL P/N: BH-B500-710; BOHMER; BLOCK","Bohmer","BALL","10 MM","STEEL","500 LB","BALL STL","FNPT","N/S","N/S","LEVER","High-pressure process fluid service","150 deg","BH-B500-710"]
["Drakensberg Pumped Storage Scheme",72006,"VALVE, BALL: VALVE SIZE: DN 65 MM; DESIGN RATING: PN100; CONNECTION: FLANGE; REFERENCE NO: 3121-0065-530401; SHUT OFF; COMPLETE WITH HANDLE 350 K","Bohmer","BALL","DN 65 MM","STEEL","PN100","N/S","FLANGE","N/S","N/S","HAND","Shut-off/isolation service","150 deg","3121-0065-530401"]
["Drakensberg Pumped Storage Scheme",72007,"VALVE, BALL: VALVE SIZE: 16 MM; DESIGN RATING: 400 LB; CONNECTION: NPT; BODY MATERIAL: STEEL; OPERATED: LEVER; STYLE: 2 WAY; TRIM: BALL STL; BOHMER BLOCK","Bohmer","BALL","16 MM","STEEL","400 LB","BALL STL","NPT","95 mm","N/S","LEVER","Process fluid isolation/shut-off service","150 deg"]
["Drakensberg Pumped Storage Scheme",72008,"VALVE, BALL: VALVE SIZE: 10 MM; DESIGN RATING: 315; CONNECTION: NPT; BODY MATERIAL: STEEL; OPERATED: LEVER; STYLE: 4 WAY; TRIM: BALL STL; SUPPL P/N: VH-VX315-210; REFERENCE NO: VX315-210; BOHMER; BLOCK","Bohmer","BALL","10 MM","STEEL",315,"BALL STL","NPT","N/S","N/S","LEVER","Process fluid isolation/control service","80 deg","VH-VX315-210; VX315-210"]
["Drakensberg Pumped Storage Scheme",72014,"VALVE, BALL: VALVE SIZE: 20 MM; DESIGN RATING: 315; CONNECTION: NPT; BODY MATERIAL: STEEL; OPERATED: LEVER; STYLE: 2 WAY; TRIM: BALL STL; BLOCK; BOHMER","Bohmer","BALL","20 MM","STEEL",315,"BALL STL","NPT","95 mm","N/S","LEVER","Process fluid isolation/shut-off service","80 deg"]
["Drakensberg Pumped Storage Scheme",72026,"VALVE, RELIEF: VALVE SIZE: 13 MM; SET PRESSURE: 240 LB; CONNECTION: NPT; BODY MATERIAL: BRASS; TRIM: DISC BRS; SPRING STL; OPERATED: PRESSURE, SPRING; SUPPL P/N: 98650/1172; SECOND STAGE SAFETY","Haskel Energy Systems (probable)","RELIEF","13 MM","BRASS","240 LB","DISC BRS","NPT","50 mm","N/S","PRESSURE, SPRING","Pressure relief service","80 deg","98650/1172"]
["Drakensberg Pumped Storage Scheme",72016,"VALVE, BALL: VALVE SIZE: 8 MM; DESIGN RATING: 500 LB; CONNECTION: FNPT; BODY MATERIAL: STEEL; OPERATED: LEVER; STYLE: 2 WAY; TRIM: BALL STL; BOHMER; BLOCK","Bohmer","BALL","8 MM","STEEL","500 LB","BALL STL","FNPT","95 mm","N/S","LEVER","Process fluid isolation/shut-off service","150 deg"]
["Drakensberg Pumped Storage Scheme",72017,"VALVE, BALL: VALVE SIZE: 6 MM; DESIGN RATING: 500 LB; CONNECTION: FNPT; BODY MATERIAL: STEEL; OPERATED: LEVER; STYLE: 2 WAY; TRIM: BALL STL; BOHMER; BLOCK","Bohmer","BALL","6 MM","STEEL","500 LB","BALL STL","FNPT","95 mm","N/S","LEVER","Process fluid isolation/shut-off service","150 deg"]
["Drakensberg Pumped Storage Scheme",72018,"VALVE, GLOBE: VALVE SIZE: 4 MM; OPERATED: HANDWHEEL; CONNECTION: NPT; BODY MATERIAL: STL A122; TRIM: SPINDLE 4122; STEM DESIGN: INSIDE SCREW; STYLE: THD BONNET; DESIGN RATING: 400 BAR; ERMETO HIGH PRESSURE; TUBE SIZE OD 8 MM","Parker Hannifin (Ermeto)","GLOBE","4 MM","STL A122","400 BAR","SPINDLE 4122; INSIDE SCREW","NPT","P2 handwheel","N/S","HANDWHEEL","High-pressure instrumentation / hydraulic service","150 deg"]
["Drakensberg Pumped Storage Scheme",72020,"VALVE, CHECK: TYPE: PISTON; VALVE SIZE: 12 MM; CONNECTION: FNPT; BODY MATERIAL: STL; STYLE: THD CAP; TRIM: DISC STL; BRAKE AIR COMPRESS","Parker Hannifin (probable)","CHECK; PISTON","12 MM","STL","N/S","DISC STL","FNPT","190 mm","N/S","PRESSURE","Brake air compressor service","150 deg"]
["Drakensberg Pumped Storage Scheme",72021,"VALVE, RELIEF: VALVE SIZE: 12 MM; CONNECTION: NPT; BODY MATERIAL: STL; TRIM: SPRING STL; OPERATED: PRESSURE, SPRING; REFERENCE NO: 98650-1162; OIL REGULATOR","Haskel Energy Systems","RELIEF","12 MM","STL","N/S","SPRING STL","NPT","2N12 mm","N/S","PRESSURE, SPRING","Oil regulator service","80 deg","98650-1162"]
["Drakensberg Pumped Storage Scheme",72022,"VALVE, RELIEF: VALVE SIZE: 12 MM; SET PRESSURE: 42 LB; CONNECTION: NPT; BODY MATERIAL: BRASS; TRIM: DISC BRS; SPRING STL; OPERATED: PRESSURE, SPRING; SUPPL P/N: 98650/1171; FIRST STAGE SAFETY; SEETRU; 311100200 C1940","Seetru Limited","RELIEF","12 MM","BRASS","42 LB","DISC BRS","NPT","5; mm","N/S","PRESSURE, SPRING","Safety pressure relief service","80 deg","98650/1171"]
["Drakensberg Pumped Storage Scheme",72023,"VALVE: TYPE: DISCHARGE; VALVE SIZE: 51 MM; OPERATED: PRESSURE; BODY MATERIAL: STL; TRIM: DISC STL; SUPPL P/N: 98650/1180; CONNECTION COMPRESSION; FIRST STAGE DELIVERY","Haskel Energy Systems","DISCHARGE","51 MM","STL","N/S","DISC STL","COMPRESSION","4D: PRESSURE; e-to-Face, Drilling / PCD, Mediume-to-Face, Drilling / PCD, Medium","N/S","PRESSURE","First stage delivery/discharge service","120 deg","98650/1180"]
["Drakensberg Pumped Storage Scheme",72024,"VALVE: TYPE: COMPRESSOR; VALVE SIZE: 8 MM; CONNECTION: THD FEMALE; OPERATED: PRESSURE; BODY MATERIAL: STL; STYLE: 6 WAY; TRIM: BONNET/DISC STL; REFERENCE NO: 98650-1161; 4TH STAGE; SIZE 11MM THK","Haskel Energy Systems","COMPRESSOR","8 MM","STL","N/S","BONNET/DISC STL","THD FEMALE","2 lve size: 8 mm; connection: thd female; operated: pressure; body material: stl","N/S","PRESSURE","Compressor stage service","180 deg","98650-1161"]
["Drakensberg Pumped Storage Scheme",72027,"VALVE, RELIEF: VALVE SIZE: 13 MM; SET PRESSURE: 1160 LB; CONNECTION: NPT; BODY MATERIAL: BRASS; TRIM: DISC BRS; SPRING STL; OPERATED: PRESSURE, SPRING; SUPPL P/N: 98650/1173; THIRD STAGE SAFETY; SEETRU","Seetru Limited","RELIEF","13 MM","BRASS","1160 LB","DISC BRS","NPT","560 mm","N/S","PRESSURE, SPRING","High-pressure safety relief service","150 deg","98650/1173"]
["Drakensberg Pumped Storage Scheme",72029,"VALVE: TYPE: DISCHARGE; VALVE SIZE: 34 MM; CONNECTION: COMPRESSION; OPERATED: PRESSURE; BODY MATERIAL: MS; TRIM: DISC STL; SUPPL P/N: 98650/1182; SECOND STAGE DELIVERY","Haskel Energy Systems","DISCHARGE","34 MM","Not specified","N/S","DISC STL","COMPRESSION","2Dve size: 34 mm; connection: compression","N/S","PRESSURE","Second stage delivery/discharge service","140 deg","98650/1182"]
["Drakensberg Pumped Storage Scheme",72030,"HOUSING: TYPE: VALVE; DIMENSIONS: DIA 34 X LG 62 MM; MATERIAL: ALUMINIUM; REFERENCE NO: C200604; SECOND STAGE, COVER; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Haskel Energy Systems","VALVE","3.5 MM","ALUMINIUM","N/S","N/S","TBC","N/S","N/S","TBC","Second stage valve assembly component","150 deg","C200604"]
["Drakensberg Pumped Storage Scheme",72031,"VALVE: TYPE: COMPRESSOR; VALVE SIZE: 9 MM; CONNECTION: THD FEMALE; OPERATED: PRESSURE; STYLE: 4 WAY; TRIM: DISC STL; SUPPL P/N: 98650/1160; THIRD STAGE VALVE; SIZE 12MM LG X 14MM THK","Haskel Energy Systems","COMPRESSOR","9 MM","STEYP","N/S","DISC STL","THD FEMALE","4ION: THD -to-Face, Drilling / PCD, Medium-to-Face, Drilling / PCD, Medium","N/S","PRESSURE","Compressor stage service","180 deg","98650/1160"]
["Drakensberg Pumped Storage Scheme",72032,"VALVE, RELIEF: VALVE SIZE: 13 MM; SET PRESSURE: 138 BAR; CONNECTION: NPT; BODY MATERIAL: STAINLESS STEEL; TRIM: BONNET SS; SPRING STL; OPERATED: PRESSURE; SUPPL P/N: 98661/1011","Haskel Energy Systems","RELIEF","13 MM","STAINLESS STEEL","138 BAR","BONNET SS","NPT","58 mm","N/S","PRESSURE","High-pressure pressure relief service","80 deg","98661/1011"]
["Drakensberg Pumped Storage Scheme",72033,"VALVE, RELIEF: VALVE SIZE: 12 MM; CONNECTION: NPT; BODY MATERIAL: STAINLESS STEEL; TRIM: SPRING STL; OPERATED: PRESSURE, SPRING; SUPPL P/N: 98261/1594/1525; SAFETY; OLD S P/N 98661/1010","Haskel Energy Systems","RELIEF","12 MM","STAINLESS STEEL","N/S","SPRING STL","NPT","2E12 mm","N/S","PRESSURE, SPRING","Safety pressure relief service","80 deg","98261/1594/1525"]
["Drakensberg Pumped Storage Scheme",72034,"VALVE, RELIEF: VALVE SIZE: 34 MM; CONNECTION: FLANGE; BODY MATERIAL: CI; TRIM: SPRING STL; OPERATED: PRESSURE, SPRING; ITEM 20","HEROSE (probable)","RELIEF","34 MM","CI","N/S","SPRING STL","FLANGE","2R34 mm","N/S","PRESSURE, SPRING","Pressure relief service","80 deg"]
["Drakensberg Pumped Storage Scheme",72035,"VALVE, RELIEF: REFERENCE NO: L16; L-16; 503D","Haskel Energy Systems (probable)","RELIEF","N/S","STEEL","N/S","N/S","TBC","N/S","N/S","PRESSURE","Pressure relief servic","80 deg","L16"]
["Drakensberg Pumped Storage Scheme",72036,"VALVE, CHECK: VALVE SIZE: 14 X 12 MM; CONNECTION: NPT; BODY MATERIAL: BRASS; STYLE: THD CAP; TRIM: CAP/SLEEVE BRS; SUPPL P/N: SCD-6504; 633; MODEL NO: 5H12; REFERENCE NO: PT633; 32001117; TYPE LIFT; WITH SLEEVE AND 12.7MM NUT; FOR INGERSOL FIRE PROTECTION COMPRESSOR","LIFT","CHECK","14 X 12 MM","BRASS","N/S","CAP/SLEEVE BRS","NPT","95 mm","N/S","PRESSURE","compressed air/gas service","80 deg","SCD-6504; PT633; 5H12"]
["Drakensberg Pumped Storage Scheme",72037,"VALVE: TYPE: BARE; VALVE SIZE: 48 MM; CONNECTION: FLANGE; OPERATED: PRESSURE; BODY MATERIAL: STAINLESS STEEL; TRIM: PLATE SS; REFERENCE NO: 1-32; 1095","Haskel Energy Systems (probable)","BARE","48 MM","STAINLESS STEEL","N/S","PLATE SS","FLANGE","2Mze: 48 mm; connection: flange","N/S","PRESSURE","Pressure operated valve service","150 deg","1932-01-01"]
["Drakensberg Pumped Storage Scheme",72038,"VALVE, GLOBE: VALVE SIZE: 3 IN; OPERATED: HANDWHEEL; CONNECTION: FLANGE; BODY MATERIAL: CS; TRIM: DISC/SEAT 13CR; GRADE: WCB; STEM DESIGN: RISING OUTSIDE SCREW; STYLE: BOLTED BONNET; DESIGN RATING: 150 LB; REFERENCE NO: 2H18802; HIRATA","Hirata","GLOBE","3 IN","CS","150 LB","DISC/SEAT 13CR; RISING OUTSIDE SCREW","FLANGE","SCREW; STYLE: BOLTED BONNET; DESIGN RATING: 150 LB; REFERENCE NO: 2SCREW; STYLE: BOLTED BONNET; DESIGN RATING: 150 LB; REFERENCE NO: 2 mm","N/S","HANDWHEEL","Isolation/control service","200 deg","2H18802",null,"R"]
["Drakensberg Pumped Storage Scheme",72039,"VALVE, GLOBE: VALVE SIZE: 4 IN; OPERATED: HANDWHEEL; CONNECTION: FLANGE; BODY MATERIAL: CS; TRIM: SEAT 13CR; GRADE: WCB; STEM DESIGN: INSIDE SCREW; STYLE: BOLTED BONNET; DESIGN RATING: 150 LB; REFERENCE NO: 2H18629; HIRATA","Hirata","GLOBE","4 IN","CS","150 LB","SEAT 13CR; INSIDE SCREW","FLANGE","N/S","N/S","HANDWHEEL","Isolation/control service","200 deg","2H18629",null,"R"]
["Drakensberg Pumped Storage Scheme",72040,"VALVE, GATE: VALVE SIZE: 3 IN; TYPE: SOLID WEDGE; CONNECTION: FLANGE; BODY MATERIAL: STEEL; TRIM: SEAT 13CR; OPERATED: HANDWHEEL; STEM DESIGN: RISING OUTSIDE SCREW; STYLE: BOLTED BONNET; GRADE: WCB; DESIGN RATING: 150 LB; REFERENCE NO: 2H27347; CAST; HIRATA","Hirata","GATE; SOLID WEDGE","3 IN","STEEL","150 LB","SEAT 13CR; RISING OUTSIDE SCREW","FLANGE","210 mm","N/S","HANDWHEEL","Isolation service","200 deg","2H27347",null,"R"]
["Drakensberg Pumped Storage Scheme",72041,"VALVE, GLOBE: VALVE SIZE: 2 IN; OPERATED: HANDWHEEL; CONNECTION: FLANGE; BODY MATERIAL: CS; TRIM: DISC 13CR; GRADE: WCB; STEM DESIGN: RISING OUTSIDE SCREW; STYLE: BOLTED BONNET; DESIGN RATING: 600 LB; DRAWING NO: 2H18630 REV 1; HIRATA; SIZE 50 MM","Hirata","GLOBE","2 IN","CS","600 LB","DISC 13CR; RISING OUTSIDE SCREW","FLANGE","N/S","N/S","HANDWHEEL","Isolation/control service","250 deg","2H18630 REV 1"]
["Drakensberg Pumped Storage Scheme",72042,"VALVE, CHECK: VALVE SIZE: 2 IN; DESIGN RATING: 600 LB; CONNECTION: FLANGE; BODY MATERIAL: CS; DRAWING NO: 2H33514 REV 1; TYPE LIFT; HIRATA","LIFT; Hirata","CHECK","2 IN","CS","600 LB","Stainless steel 410 (AISI 410 SS) or 316 SS (depending on service)","FLANGE","N/S","N/S","PRESSURE","Flow control / backflow prevention service","250 deg","2H33514 REV 1"]
["Drakensberg Pumped Storage Scheme",72043,"VALVE, GLOBE: VALVE SIZE: 10 MM; OPERATED: HANDWHEEL; CONNECTION: FNPT; BODY MATERIAL: STL FORGED; TRIM: SEAT 13CR; STEM DESIGN: RISING OUTSIDE SCREW; STYLE: BOLTED BONNET; DESIGN RATING: 150-800 LB; DRAWING NO: 2N18553 REV 1; HIRATA","Hirata","GLOBE","10 MM","STL FORGED","150-800 LB","SEAT 13CR; RISING OUTSIDE SCREW","FNPT","1008 mm","N/S","HANDWHEEL","Isolation/control service","300 deg","2N18553 REV 1",null,"R"]
["Drakensberg Pumped Storage Scheme",72044,"VALVE, GATE: VALVE SIZE: 1/2 IN; TYPE: WEDGE; CONNECTION: THD TAPER FEMALE; BODY MATERIAL: BRS CAST; TRIM: BRASS; OPERATED: HANDWHEEL; STEM DESIGN: NON RISING; STYLE: THD BONNET; SPECIFICATION: SABS 776; DESIGN RATING: 1600 KPA; TEMP RATING 880 KPA AT 175 DEG C; FULLWAY; CLASS 8; BONNET TYPE HEAD; GUIDED; WORKING PRESSURE 880 KPA AT 100 DEG C; HYDRAULIC WORKING PRESSURE 1600 KPA; TESTED TO 2000 KPA; BEARING THE SABS MARK OF APPROVAL","HEAD","GATE; WEDGE","1/2 IN","BRS CAST","1600 KPA","BRASS; NON RISING","THD TAPER FEMALE","N/S","N/S","HANDWHEEL","Isolation service","100 deg"]
["Drakensberg Pumped Storage Scheme",72045,"VALVE, GLOBE: VALVE SIZE: 4 IN; OPERATED: HANDWHEEL; CONNECTION: FLANGE; BODY MATERIAL: CS; TRIM: SEAT 13CR; GRADE: WCB; STEM DESIGN: RISING OUTSIDE SCREW; STYLE: BOLTED BONNET; DESIGN RATING: 150 LB; REFERENCE NO: 2H18803; 4820-70-5093043; HIRATA; SIZE: 100 MM","Hirata","GLOBE","4 IN","CS","150 LB","SEAT 13CR; RISING OUTSIDE SCREW","FLANGE","N/S","N/S","HANDWHEEL","Isolation/control service","200 deg","2H18803",null,"R"]
["Drakensberg Pumped Storage Scheme",72046,"VALVE, GATE: VALVE SIZE: 2-1/2 IN; CONNECTION: FLANGE; BODY MATERIAL: CS; DESIGN RATING: 150 LB; DRAWING NO: 2H27346 REV 1","Hopkinsons Valve (probable)","GATE","2-1/2 IN","CS","150 LB","N/S","FLANGE","190 mm","N/S","HANDWHEEL","Isolation service","200 deg","2H27346 REV 1"]
["Drakensberg Pumped Storage Scheme",72047,"VALVE, GATE: VALVE SIZE: 5 IN; CONNECTION: FLANGE; BODY MATERIAL: CS; TRIM: BONNET STL; OPERATED: HANDWHEEL; STEM DESIGN: RISING OUTSIDE SCREW; STYLE: BOLTED BONNET; DESIGN RATING: 150 LB; REFERENCE NO: 2H27348; HIRATA","Hirata","GATE","5 IN","CS","150 LB","BONNET STL; RISING OUTSIDE SCREW","FLANGE","N/S","N/S","HANDWHEEL","Isolation service","200 deg","2H27348"]
["Drakensberg Pumped Storage Scheme",72048,"VALVE, GATE: VALVE SIZE: 150 MM; CONNECTION: FLANGE; BODY MATERIAL: CS; TRIM: SEAT 13CR; OPERATED: HANDWHEEL; STEM DESIGN: RISING OUTSIDE SCREW; STYLE: BOLTED BONNET; GRADE: WCB; DESIGN RATING: 150 LB; REFERENCE NO: 2H27349; HIRATA","Hirata","GATE","150 MM","CS","150 LB","SEAT 13CR; RISING OUTSIDE SCREW","FLANGE","N/S","N/S","HANDWHEEL","Isolation service","200 deg","2H27349",null,"R"]
["Drakensberg Pumped Storage Scheme",72059,"VALVE, GLOBE: VALVE SIZE: 1/2 IN; OPERATED: HANDWHEEL; CONNECTION: FNPT; BODY MATERIAL: STEEL; TRIM: DISC/SEAT SS GR 316; STEM DESIGN: INSIDE SCREW; STYLE: THD BONNET; DESIGN RATING: 150-200 LB; DRAWING NO: 2S18669 REV 1; HIRATA; MATERIAL SUSF316-97","Hirata","GLOBE","1/2 IN","STEEL","150-200 LB","DISC/SEAT SS GR 316; INSIDE SCREW","FNPT","N/S","N/S","HANDWHEEL","Isolation/control service","200 deg","2S18669 REV 1",null,6]
["Drakensberg Pumped Storage Scheme",72050,"VALVE, ANGLE: TYPE: NEEDLE; VALVE SIZE: 200 MM; DESIGN RATING: 300 LB; CONNECTION: FLANGE; BODY MATERIAL: STL CAST; OPERATED: HANDWHEEL, GEAR; STYLE: BOLTED BONNET; TRIM: BONNET/DISC STL; GRADE: WCB 8B; DRAWING NO: HIRATA 2H18923 REV 1; REFERENCE NO: 2H18923","Hirata","ANGLE; NEEDLE","200 MM","STL CAST","300 LB","BONNET/DISC STL","FLANGE","95 mm","N/S","HANDWHEEL, GEAR","Flow regulation/isolation service","250 deg","2H18923; HIRATA 2H18923 REV 1"]
["Drakensberg Pumped Storage Scheme",72052,"VALVE, GATE: VALVE SIZE: 50 MM; TYPE: SOLID WEDGE; CONNECTION: FLANGE; BODY MATERIAL: STEEL; TRIM: DISC 13CR; OPERATED: HANDWHEEL; STEM DESIGN: RISING OUTSIDE SCREW; STYLE: BOLTED BONNET; GRADE: WCB; DESIGN RATING: 600 LB; REFERENCE NO: 2H27350; CAST; HIRATA","Hirata","GATE; SOLID WEDGE","50 MM","STEEL","600 LB","DISC 13CR; RISING OUTSIDE SCREW","FLANGE","260 mm","N/S","HANDWHEEL","Isolation service","300 deg","2H27350"]
["Drakensberg Pumped Storage Scheme",72053,"VALVE, GATE: VALVE SIZE: 3 IN; TYPE: SOLID WEDGE; CONNECTION: FLANGE; BODY MATERIAL: STEEL; TRIM: SEAT 13CR; OPERATED: HANDWHEEL; STEM DESIGN: RISING OUTSIDE SCREW; STYLE: BOLTED BONNET; GRADE: WCB; DESIGN RATING: 600 LB; REFERENCE NO: 2H27351; CAST; HIRATA","Hirata","GATE; SOLID WEDGE","3 IN","STEEL","600 LB","SEAT 13CR; RISING OUTSIDE SCREW","FLANGE","260 mm","N/S","HANDWHEEL","Isolation service","300 deg","2H27351",null,"R"]
["Drakensberg Pumped Storage Scheme",72054,"VALVE, GLOBE: VALVE SIZE: 100 MM; OPERATED: HANDWHEEL; CONNECTION: FLANGE; BODY MATERIAL: CS; TRIM: SEAT 13CR; GRADE: WCB; STEM DESIGN: RISING OUTSIDE SCREW; STYLE: BOLTED BONNET; DESIGN RATING: 600 LB; REFERENCE NO: 2H18626; HIRATA","Hirata","GLOBE","100 MM","CS","600 LB","SEAT 13CR; RISING OUTSIDE SCREW","FLANGE","N/S","N/S","HANDWHEEL","Isolation/control service","300 deg","2H18626",null,"R"]
["Drakensberg Pumped Storage Scheme",72055,"VALVE, CHECK: TYPE: SWING; VALVE SIZE: 100 MM; DESIGN RATING: 600 LB; CONNECTION: FLANGE; BODY MATERIAL: CS; STYLE: BOLTED CAP; TRIM: BONNET STL; REFERENCE NO: 2H33536; HIRATA","Hirata","CHECK; SWING","100 MM","CS","600 LB","BONNET STL","FLANGE","N/S","N/S","PRESSURE","Backflow prevention service","300 deg","2H33536"]
["Drakensberg Pumped Storage Scheme",72056,"VALVE, GATE: VALVE SIZE: 1/2 IN; TYPE: SOLID WEDGE; CONNECTION: FLANGE; BODY MATERIAL: STEEL; TRIM: SEAT 13CR; OPERATED: HANDWHEEL; STEM DESIGN: INSIDE SCREW; STYLE: BOLTED BONNET; DESIGN RATING: 150-800 LB; REFERENCE NO: 2M27352; FORGED; HIRATA","Hirata","GATE; SOLID WEDGE","1/2 IN","STEEL","150-800 LB","SEAT 13CR; INSIDE SCREW","FLANGE","210-800 mm","N/S","HANDWHEEL","Isolation service","350 deg","2M27352",null,"R"]
["Drakensberg Pumped Storage Scheme",72057,"VALVE, GATE: VALVE SIZE: 100 MM; CONNECTION: FLANGE; BODY MATERIAL: CS; DESIGN RATING: 150 LB; REFERENCE NO: 2H27354; HIRATA","Hirata","GATE","100 MM","CS","150 LB","N/S","FLANGE","230 mm","N/S","HANDWHEEL","Isolation service","200 deg","2H27354"]
["Drakensberg Pumped Storage Scheme",72058,"VALVE, GATE: VALVE SIZE: 3/8 IN; TYPE: SOLID WEDGE; CONNECTION: FNPT; BODY MATERIAL: STEEL; TRIM: SEAT 13CR; OPERATED: HANDWHEEL; STEM DESIGN: RISING OUTSIDE SCREW; STYLE: BOLTED BONNET; DESIGN RATING: 600 LB; DRAWING NO: 2N27361 REV 1; FORGED; HIRATA","Hirata","GATE; SOLID WEDGE","3/8 IN","STEEL","600 LB","SEAT 13CR; RISING OUTSIDE SCREW","FNPT","260 mm","N/S","HANDWHEEL","Isolation service","350 deg","2N27361 REV 1",null,"R"]
["Drakensberg Pumped Storage Scheme",72060,"VALVE, GLOBE: VALVE SIZE: 10 MM; OPERATED: HANDWHEEL; CONNECTION: FNPT; BODY MATERIAL: SS FORGED; TRIM: SEAT 13CR; STEM DESIGN: RISING OUTSIDE SCREW; STYLE: BOLTED BONNET; DESIGN RATING: 150 LB; DRAWING NO: 2S18670 REV 1; 3/8 INCH; HIRATA","Hirata","GLOBE","10 MM","SS FORGED","150 LB","SEAT 13CR; RISING OUTSIDE SCREW","FNPT","N/S","N/S","HANDWHEEL","Isolation/control service","300 deg","2S18670 REV 1",null,"R"]
["Drakensberg Pumped Storage Scheme",72061,"VALVE, GLOBE: VALVE SIZE: 25 MM; OPERATED: HANDWHEEL; CONNECTION: FLANGE; BODY MATERIAL: STEEL; TRIM: DISC/SEAT 13CR; STEM DESIGN: RISING OUTSIDE SCREW; STYLE: BOLTED BONNET; DESIGN RATING: 150-800 LB; FUJITAT-210","Fujikin Incorporated (probable)","GLOBE","25 MM","STEEL","150-800 LB","DISC/SEAT 13CR; RISING OUTSIDE SCREW","FLANGE","TBC","N/S","HANDWHEEL","Isolation/control service","200 deg",null,null,"R"]
["Drakensberg Pumped Storage Scheme",72062,"VALVE, GLOBE: VALVE SIZE: 1/2 IN; OPERATED: HANDWHEEL; CONNECTION: FLANGE; BODY MATERIAL: STL FORGED; TRIM: SEAT 13CR; STEM DESIGN: INSIDE SCREW; STYLE: BOLTED BONNET; DESIGN RATING: 150-800 LB; DRAWING NO: 2M18627 REV 1; HIRATA","Hirata","GLOBE","1/2 IN","STL FORGED","150-800 LB","SEAT 13CR; INSIDE SCREW","FLANGE","108 mm","N/S","HANDWHEEL","Isolation/control service","−29 to 425 deg","2M18627 REV 1",null,"R"]
["Drakensberg Pumped Storage Scheme",72063,"VALVE, GLOBE: VALVE SIZE: 3 IN; OPERATED: HANDWHEEL; CONNECTION: FLANGE; BODY MATERIAL: CS; TRIM: SEAT 13CR; GRADE: WCB; STEM DESIGN: RISING OUTSIDE SCREW; STYLE: BOLTED BONNET; DESIGN RATING: 600 LB; DRAWING NO: 952-230003 REV 1; KITAZAWA","Kitazawa Valve Co., Ltd.","GLOBE","3 IN","CS","600 LB","SEAT 13CR; RISING OUTSIDE SCREW","FLANGE","N/S","N/S","HANDWHEEL","Isolation/control service","−29 to 425 deg","952-230003 REV 1",null,"R"]
["Drakensberg Pumped Storage Scheme",73053,"VALVE, BUTTERFLY: TYPE: WAFER; VALVE SIZE: 75 MM; DESIGN RATING: 740 LB; TEMPERATURE RATING: -250 TO 500 DEG F; CONNECTION: FLANGE; BODY MATERIAL: STAINLESS STEEL; TRIM: DISC SS GR 316; ELECTRICAL; MINITORK ASSY TURB","Minitork (actuator/assembly)","BUTTERFLY; WAFER","75 MM","STAINLESS STEEL","740 LB","DISC SS GR 316","FLANGE","43 mm","N/S","HANDWHEEL","Isolation/throttling service","-250 TO 500 DEG F"]
["Drakensberg Pumped Storage Scheme",75280,"VALVE, RELIEF: SET PRESSURE: 150 LB; CONNECTION: THD; BODY MATERIAL: BRASS; TRIM: CU; OPERATED: SPRING; SUPPL P/N: X1396T28-160; MODEL NO: 41; SAFETY; FOR INGERSOLL RAND COMPRESSOR; TYPE 30","Ingersoll Rand","RELIEF","N/S","BRASS","150 LB","CU","THD","N/S","N/S","SPRING","Compressor safety relief service","−29 to 204 deg","X1396T28-160; 41"]
["Drakensberg Pumped Storage Scheme",77118,"VALVE, RELIEF: VALVE SIZE: 1/4 IN; SET PRESSURE: 60 LB; CONNECTION: NPT; BODY MATERIAL: BRASS; TRIM: SPRING STL; STEM BRS; OPERATED: PRESSURE, SPRING; SUPPL P/N: 3W123 662T2; STOP","Haskel Energy Systems (probable)","RELIEF","1/4 IN","BRASS","60 LB","SPRING STL","NPT","50 mm","N/S","PRESSURE, SPRING","Pressure relief / stop service","−29 to 200 deg","3W123 662T2"]
["Drakensberg Pumped Storage Scheme",77123,"VALVE: TYPE: INLET; VALVE SIZE: 27 MM; CONNECTION: COMPRESSION; OPERATED: PRESSURE; BODY MATERIAL: STL; TRIM: DISC STL; SUPPL P/N: 11458-8K1N 30220453; REFERENCE NO: 11458-8K1N; 30220453; COMPLETE; FOR TYPE 30 MOD41 ING-RAND AIR COMPRESSOR; 20.4MM THK","Ing-Rand","INLET","27 MM","STL","N/S","DISC STL","COMPRESSION","FERENCE NO: 11458-8K1FERENCE NO: 11458-8K1 ing / PCD, Mediuming / PCD, Medium","N/S","PRESSURE","Air compressor inlet service","−29 to 200 deg","11458-8K1N 30220453; 11458-8K1N"]
["Drakensberg Pumped Storage Scheme",77124,"VALVE: TYPE: DISCHARGE; VALVE SIZE: 27 MM; CONNECTION: COMPRESSION; OPERATED: PRESSURE; BODY MATERIAL: STL; TRIM: DISC STL; REFERENCE NO: 30279459","Burckhardt Compression","DISCHARGE","27 MM","STL","N/S","DISC STL","COMPRESSION","7 ve size: 27 mm","N/S","PRESSURE","Air compressor discharge service","150–200 deg",30279459]
["Drakensberg Pumped Storage Scheme",77126,"VALVE: TYPE: INLET; SUPPL P/N: 8K6N; STOP PLATE; FOR TYPE 30 MODEL 41 ING-RAND COMPRESSOR","FOR TYPE 30; Ing-Rand","INLET","N/S","STEYP","N/S","N/S","COMPRESSION","N/S","N/S","PRESSURE","Air compressor inlet valve service","−29 to 200 deg","8K6N"]
["Drakensberg Pumped Storage Scheme",77130,"CAP: TYPE: VALVE CAGE; DIMENSIONS: DIA 85 X HT 38 MM; MATERIAL: STL; SUPPL P/N: 3W75340; MODEL NO: 41 TYPE 30; FOR 22K AIR HEAD ASSEMBLY","Haskel","VALVE CAGE","85 MM","STL","N/S","N/S","TBC","N/S","N/S","TBC","Air compressor valve assembly service","−29 to 200 deg","3W75340; 41 TYPE 30"]
["Drakensberg Pumped Storage Scheme",77133,"VALVE, RELIEF: VALVE SIZE: 22 X 11 MM; CONNECTION: NPT; BODY MATERIAL: ALUMINIUM; TRIM: SPRING STL; OPERATED: PRESSURE, SPRING; REFERENCE NO: 3R53608T50; PRESSURE; ING-RAND","Ing-Rand","RELIEF","22 X 11 MM","ALUMINIUM","N/S","SPRING STL","NPT","N/S","N/S","PRESSURE, SPRING","Air compressor pressure relief service","−29 to 150 deg","3R53608T50"]
["Drakensberg Pumped Storage Scheme",77134,"VALVE, RELIEF: VALVE SIZE: 1/4 IN; SET PRESSURE: 1300 LB; CONNECTION: NPT; BODY MATERIAL: BRASS; TRIM: SPRING STL; OPERATED: PRESSURE, SPRING; MODEL NO: 15T2; REFERENCE NO: X1396T19-1300; SAFETY; FOR TYPE 30; ING-RAND COMPRESSOR","Ing-Rand","RELIEF","1/4 IN","BRASS","1300 LB","SPRING STL","NPT","55 mm","N/S","PRESSURE, SPRING","Air compressor safety relief service","−29 to 200 deg","X1396T19-1300; 15T2"]
["Drakensberg Pumped Storage Scheme",77135,"VALVE, RELIEF: VALVE SIZE: 1/4 IN; SET PRESSURE: 60 LB; CONNECTION: NPT; BODY MATERIAL: BRASS; TRIM: DISC BRS; SPRING STL; OPERATED: PRESSURE, SPRING; MODEL NO: 15T2; REFERENCE NO: X1396T28-60LB; COMPRESSOR 1ST STAGE INTERCOOLER SAFETY; FOR TYPE 30; AIR COMPRESSOR","Haskel","RELIEF","1/4 IN","BRASS","60 LB","DISC BRS","NPT","95 in","N/S","PRESSURE, SPRING","Compressor intercooler safety relief service","−29 to 200 deg","X1396T28-60LB; 15T2"]
["Drakensberg Pumped Storage Scheme",77136,"VALVE, RELIEF: VALVE SIZE: 1/4 IN; SET PRESSURE: 260 LB; CONNECTION: NPT; BODY MATERIAL: BRASS; TRIM: STEM BRS; SPRING STL; OPERATED: PRESSURE, SPRING; REFERENCE NO: X1396T28-260LB; 2ND STAGE INTERCOOLER SAFETY; FOR TYPE 30 MODEL 15T2 ING-RAND AIR COMPRESSOR","FOR TYPE 30; Ing-Rand","RELIEF","1/4 IN","BRASS","260 LB","STEM BRS","NPT","95 in","N/S","PRESSURE, SPRING","Compressor intercooler safety relief service","−29 to 200 deg","X1396T28-260LB"]
["Drakensberg Pumped Storage Scheme",77144,"VALVE, CHECK: VALVE SIZE: 4 IN; CONNECTION: FLANGE; BODY MATERIAL: STL; TRIM: DISC/SPRING STL; REFERENCE NO: MB8-223.2410B; MB9-642.7400; MB9-341.2400; FLOAT; DIGS","Haskel Energy Systems","CHECK","4 IN","STL","N/S","DISC/SPRING STL","FLANGE","190 mm","N/S","PRESSURE","Flow control / backflow prevention service","N/S","MB8-223.2410B"]
["Drakensberg Pumped Storage Scheme",77140,"VALVE, CHECK: SUPPL P/N: 32211724; REFERENCE NO: 49815C; CONDENSATE DRAIN; AUTOMATIC; UL104C; NOT USED W/MANUAL DRAIN VALVE; CPN","Haskel Energy Systems","CHECK","N/S","STEHE","N/S","N/S","TBC","N/S","N/S","AUTOMATIC","Compressor condensate drain service","N/S","32211724; 49815C"]
["Drakensberg Pumped Storage Scheme",77145,"VALVE, RELIEF: VALVE SIZE: 20 MM; SET PRESSURE: 60 BAR; CONNECTION: FNPT; BODY MATERIAL: BRASS; TRIM: DISC/SPRING STL; OPERATED: PRESSURE, SPRING; SAFETY PROPORTIONAL; I-R","Haskel Energy Systems","RELIEF","20 MM","BRASS","60 BAR","DISC/SPRING STL","FNPT","N/S","N/S","PRESSURE, SPRING","Pressure safety relief service","N/S"]
["Drakensberg Pumped Storage Scheme",77142,"VALVE, RELIEF: VALVE SIZE: 1/4 IN; SET PRESSURE: 1300 LB; CONNECTION: NPT; BODY MATERIAL: BRASS; TRIM: SPRING STL; STEM BRS; OPERATED: PRESSURE, SPRING; REFERENCE NO: W123662T2; SAFETY; ING-RAND","Ing-Rand","RELIEF","1/4 IN","BRASS","1300 LB","SPRING STL","NPT","N/S","N/S","PRESSURE, SPRING","Air compressor safety relief service","N/S","W123662T2"]
["Drakensberg Pumped Storage Scheme",77143,"VALVE, BALL: VALVE SIZE: 12 MM; DESIGN RATING: 250 BAR; CONNECTION: FNPT; BODY MATERIAL: STEEL; OPERATED: LEVER; STYLE: 4 WAY; TRIM: BALL STL; SUPPL P/N: VH-VX200-716; BOHMER; BLOCK","Bohmer","BALL","12 MM","STEEL","250 BAR","BALL STL","FNPT","N/S","N/S","LEVER","Isolation/diversion service","N/S","VH-VX200-716"]
["Drakensberg Pumped Storage Scheme",77146,"VALVE, BALL: VALVE SIZE: 16 MM; DESIGN RATING: 250 LB; CONNECTION: NPT; BODY MATERIAL: STEEL; OPERATED: LEVER; STYLE: 2 WAY; TRIM: BALL STL; SUPPL P/N: BH-B400-216; BLOCK; BOHMER","Bohmer","BALL","16 MM","STEEL","250 LB","BALL STL","NPT","N/S","N/S","LEVER","Isolation service","N/S","BH-B400-216"]
["Drakensberg Pumped Storage Scheme",77148,"VALVE, BALL: VALVE SIZE: 20 MM; DESIGN RATING: 200 BAR; CONNECTION: FNPT; BODY MATERIAL: BRZ; OPERATED: LEVER; STYLE: 4 WAY; TRIM: BALL BRZ; SOFTGOODS: SEAL JOINT TEFLON; BOHMER; BLOCK.","Bohmer","BALL","20 MM","BRZ","200 BAR","BALL BRZ","FNPT","95 mm","N/S","LEVER","Isolation/diversion service","N/S",null,null,"SEAL JOINT TEFLON"]
["Drakensberg Pumped Storage Scheme",77149,"VALVE, SOLENOID: PIPE SIZE: 10 MM; STYLE: 2/4 WAY; POTENTIAL: 220 VAC; DESIGN RATING: 315 BAR; BODY MATERIAL: STEEL; MEDIUM: GAS/LIQUID; POWER: 34 W; REFERENCE NO: S10G51 G019 011M; MB9-642.8800; CONNECTION MANIFOLD; OPERATION SOLENOID; GENERAL PURPOSE ENCLOSURE","Maximator","SOLENOID","10 MM","STEEL","315 BAR","N/S","Manifold mounted","190 mm","N/S","Solenoid actuated","GAS/LIQUID","N/S","S10G51 G019 011M","220 VAC; 34 W"]
["Drakensberg Pumped Storage Scheme",77150,"VALVE, CHECK: TYPE: THROTTLE; VALVE SIZE: 15 MM; CONNECTION: FNPT; BODY MATERIAL: STL; STYLE: THD CAP; TRIM: DISC/SPRING STL; DRAWING NO: MB9-642.5820 REV 1; REFERENCE NO: DDS4Q15; VOEST-ALPINE","Voestalpine","CHECK; THROTTLE","15 MM","STL","N/S","DISC/SPRING STL","FNPT","190 mm","N/S","PRESSURE","Flow control / non-return service","N/S","DDS4Q15; MB9-642.5820 REV 1"]
["Drakensberg Pumped Storage Scheme",77159,"VALVE, RELIEF: VALVE SIZE: 18 X 12 MM; SET PRESSURE: 25 BAR; CONNECTION: FNPT; BODY MATERIAL: STL; TRIM: DISC/SPRING STL; OPERATED: PRESSURE, SPRING; HAWE PRE-CONTROLLED PRESSURE CONTROL","Hawe","RELIEF","18 X 12 MM","STL","25 BAR","DISC/SPRING STL","FNPT","C7 set pressure: 25 bar","N/S","PRESSURE, SPRING","Hydraulic pressure control / relief service","N/S"]
["Drakensberg Pumped Storage Scheme",77152,"VALVE, CHECK: TYPE: THROTTLE; VALVE SIZE: 15 MM; CONNECTION: FNPT; BODY MATERIAL: STL; STYLE: THD CAP; TRIM: DISC/SPRING STL; REFERENCE NO: MB9-642-5360; DDS4Q10","Voestalpine","CHECK; THROTTLE","15 MM","STL","P/N RH18-PL","DISC/SPRING STL","FNPT","190 mm","N/S","PRESSURE, SPRING","Flow control / non-return service","N/S","MB9-642-5360"]
["Drakensberg Pumped Storage Scheme",77154,"VALVE, CHECK: TYPE: PISTON; VALVE SIZE: 18 MM; CONNECTION: NPT; BODY MATERIAL: STAINLESS STEEL; STYLE: THD CAP; TRIM: DISC/CAP SS; SUPPL P/N: RH18-PL; TUBE SIZE 18MM OD EO TUBE CONNECTION ON BOTH ENDS","Parker Hannifin","CHECK; PISTON","18 MM","STAINLESS STEEL","P/N RH18-PL","DISC/CAP SS","NPT","190 mm","N/S","PRESSURE, SPRING","Non-return service","N/S","RH18-PL"]
["Drakensberg Pumped Storage Scheme",77155,"VALVE, SOLENOID: PIPE SIZE: 10 MM; STYLE: 5 WAY; POTENTIAL: 220 VAC; DESIGN RATING: 315 BAR; BODY MATERIAL: STEEL; MEDIUM: OIL; REFERENCE NO: S10G51G020001100; 35 HZ; CONNECTION MANIFOLD; GENERAL PURPOSE ENCLOSURE; PUMP PILOT VALVE","Maximator","SOLENOID","10 MM","STEEL","315 BAR","N/S","Manifold mounted","190 mm","N/S","Solenoid actuated","OIL","N/S","S10G51G020001100","220 VAC"]
["Drakensberg Pumped Storage Scheme",77156,"VALVE, BALL: VALVE SIZE: 16 MM; DESIGN RATING: 63 LB; CONNECTION: NPT; BODY MATERIAL: STEEL; OPERATED: LEVER; STYLE: 2 WAY; TRIM: BALL STL; SUPPL P/N: BM-B63-216; BOHMER BLOCK","Bohmer","BALL","16 MM","STEEL","63 LB","BALL STL","NPT","N/S","N/S","LEVER","Isolation service","N/S","BM-B63-216"]
["Drakensberg Pumped Storage Scheme",77157,"VALVE: TYPE: EXHAUST; VALVE SIZE: 15 MM; CONNECTION: THD FEMALE; OPERATED: PRESSURE; BODY MATERIAL: ALUMINIUM; STYLE: 3 WAY; TRIM: BONNET AL; REFERENCE NO: 3340 B 10 HD-D6461; SCHOVILL SCHREIDER QUICK SHUTTLE VALVES","Schovill Schreider","EXHAUST","15 MM","ALUMINIUM","Ref. 3340 B 10 HD-D6461","BONNET AL","THD FEMALE","100 size","N/S","PRESSURE","Pneumatic exhaust/control service","N/S","3340 B 10 HD-D6461"]
["Drakensberg Pumped Storage Scheme",77160,"VALVE, SOLENOID: PIPE SIZE: 8 MM; STYLE: 4 WAY; POTENTIAL: 220 VAC; DESIGN RATING: 315 BAR; BODY MATERIAL: STEEL; OPERATED: SOLENOID; MEDIUM: GAS/LIQUID; POWER: 34 W; CAT NO: 52 012 31; REFERENCE NO: S10G51G020061300; CONNECTION MANIFOLD; GUIDE VANE TIMING CONTROL; 40 L/MIN; ENCLOSURE GENERAL PURPOSE","Maximator","SOLENOID","8 MM","STEEL","315 BAR","N/S","Manifold mounted","95 mm","N/S","SOLENOID","GAS/LIQUID","N/S","S10G51G020061300; 52 012 31","220 VAC; 34 W"]
["Drakensberg Pumped Storage Scheme",77161,"VALVE, SOLENOID: PIPE SIZE: 8 MM; STYLE: 4/2 WAY; POTENTIAL: 220 VDC; BODY MATERIAL: STEEL; MEDIUM: GAS/LIQUID; POWER: 34 W; REFERENCE NO: S10G51G0200; CONNECTION MANIFOLD; GENERAL PURPOSE ENCLOSURE; CONTROL","Maximator","SOLENOID","8 MM","STEEL","Ref. S10G51G0200","N/S","Manifold mounted","3nd Connection, Face-to-Face, Drillingnd Connection, Face-to-Face, Drilling","N/S","SOLENOID","GAS/LIQUID","N/S","S10G51G0200","220 VDC; 34 W"]
["Drakensberg Pumped Storage Scheme",77162,"VALVE, BALL: VALVE SIZE: 16 MM; DESIGN RATING: 250 LB; CONNECTION: NPT; BODY MATERIAL: BRASS; OPERATED: LEVER; STYLE: 2 WAY; TRIM: BALL STL; SUPPL P/N: BH B400-716; BOHMER; BLOCK","Bohmer","BALL","16 MM","BRASS","250 LB","BALL STL","NPT","N/S","N/S","LEVER","Isolation service","N/S","BH B400-716"]
["Drakensberg Pumped Storage Scheme",77172,"VALVE: TYPE: DIRECTIONAL; VALVE SIZE: 22 MM; OPERATED: HYDRAULIC; BODY MATERIAL: CI; STYLE: 4 WAY; TRIM: BONNET CI; DRAWING NO: K-6WO78AV8 REV 1; REFERENCE NO: DHG06/2N2/R2/40; CONNECTION MANIFOLD","Yuken","DIRECTIONAL","22 MM","CI","N/S","BONNET CI","Manifold mounted","N/S","N/S","HYDRAULIC","Hydraulic control service","N/S","DHG06/2N2/R2/40; K-6WO78AV8 REV 1"]
["Drakensberg Pumped Storage Scheme",77164,"VALVE, BALL: VALVE SIZE: 50 MM; DESIGN RATING: 64; CONNECTION: FLANGE; BODY MATERIAL: STEEL; OPERATED: LEVER; STYLE: 2 WAY; TRIM: BALL STL","Hopkinsons Valve","BALL","50 MM","STEEL",64,"BALL STL","FLANGE","95 mm","N/S","LEVER","Isolation service","N/S"]
["Drakensberg Pumped Storage Scheme",77165,"VALVE, BALL: VALVE SIZE: 25 MM; DESIGN RATING: 315 LB; CONNECTION: FNPT; BODY MATERIAL: STEEL; OPERATED: LEVER; STYLE: 2 WAY; BOHMER BLOCK","Bohmer","BALL","25 MM","STEEL","315 LB","N/S","FNPT","95 mm","N/S","LEVER","Isolation service","N/S"]
["Drakensberg Pumped Storage Scheme",77166,"VALVE, BALL: VALVE SIZE: 25 MM; DESIGN RATING: 160 LB; CONNECTION: FLANGE; BODY MATERIAL: STEEL; OPERATED: LEVER; STYLE: 2 WAY; TRIM: BALL STL; REFERENCE NO: FD; BOHMER","Bohmer","BALL","25 MM","STEEL","160 LB","BALL STL","FLANGE","95 mm","N/S","LEVER","Isolation service","N/S","FD"]
["Drakensberg Pumped Storage Scheme",77173,"VALVE, CHECK: VALVE SIZE: 30 MM; CONNECTION: FLANGE; BODY MATERIAL: CI; STYLE: THD CAP; TRIM: DISC/SHAFT STL; REFERENCE NO: SRCF10H41; TYPE LIFT; YUKEN THROTTLE","LIFT","CHECK","30 MM","CI","Ref. SRCF10H41","DISC/SHAFT STL","FLANGE","7E0 mm","N/S","PRESSURE","Hydraulic flow control / non-return service","N/S","SRCF10H41"]
["Drakensberg Pumped Storage Scheme",77169,"VALVE, GATE: VALVE SIZE: 100 MM; TYPE: SOLID WEDGE; CONNECTION: FLANGE; BODY MATERIAL: STEEL; TRIM: BONNET STL; OPERATED: HYDRAULIC; STEM DESIGN: RISING OUTSIDE SCREW; STYLE: BOLTED BONNET; DESIGN RATING: 150 LB; REFERENCE NO: 20WRC; RUNNER COOLING WATER SUPPLY AUTO","Hopkinsons Valve","GATE; SOLID WEDGE","100 MM","STEEL","150 LB","BONNET STL; RISING OUTSIDE SCREW","FLANGE","710 rilling / PCD, Mediumrilling / PCD, Medium","N/S","HYDRAULIC","Runner cooling water supply","N/S","20WRC"]
["Drakensberg Pumped Storage Scheme",77178,"JOINT, BALL: SIZE: 8 MM; CONNECTION: THD FEMALE; MATERIAL: STEEL; APPLICATION: VALVE","EMERSON","BALL","8 MM","STEEL","N/S","N/S","THD FEMALE","95 mm","N/S","TBC","VALVE","N/S"]
["Drakensberg Pumped Storage Scheme",77180,"VALVE, RELIEF: VALVE SIZE: 50 MM; SET PRESSURE: 3 KGF/CM2; CONNECTION: NPT X FNPT; BODY MATERIAL: BRASS; TRIM: SPRING STL; OPERATED: PRESSURE, SPRING; REFERENCE NO: 50-01; PT2X335L; 1ST STAGE SAFETY ASSY","CLA-VAL","RELIEF","50 MM","BRASS","3 KGF/CM2","SPRING STL","NPT X FNPT","100 mm","N/S","PRESSURE, SPRING","Safety relief service","N/S","50-01"]
["Drakensberg Pumped Storage Scheme",77183,"VALVE, RELIEF: VALVE SIZE: 32 MM; SET PRESSURE: 11.5 KG/CM2; CONNECTION: NPT X FNPT; BODY MATERIAL: BRASS; TRIM: SPRING STL; OPERATED: PRESSURE, SPRING; REFERENCE NO: HT403556; 50-02; PT11/2X275L; 2ND STAGE SAFETY","CLA-VAL","RELIEF","32 MM","BRASS","11.5 KG/CM2","SPRING STL","NPT X FNPT","5.5 mm","N/S","PRESSURE, SPRING","2nd stage safety assembly","N/S","HT403556"]
["Drakensberg Pumped Storage Scheme",77186,"VALVE, RELIEF: VALVE SIZE: 32 MM; SET PRESSURE: 11.5 KG/CM2; CONNECTION: NPT X FNPT; BODY MATERIAL: BRASS; TRIM: SPRING STL; OPERATED: PRESSURE, SPRING; REFERENCE NO: 50-03; PT3/4X210L; HT403557; 3RD STAGE SAFETY","CLA-VAL","RELIEF","32 MM","BRASS","11.5 KG/CM2","SPRING STL","NPT X FNPT","5.5 mm","N/S","PRESSURE, SPRING","3rd stage safety assembly","N/S","50-03"]
["Drakensberg Pumped Storage Scheme",77189,"VALVE, RELIEF: VALVE SIZE: 12 MM; SET PRESSURE: 8.8 KG/CM2; CONNECTION: NPT X FNPT; BODY MATERIAL: BRASS; TRIM: SPRING STL; OPERATED: PRESSURE, SPRING; REFERENCE NO: 50-04; PT3/4X280L; HT403558; 4TH STAGE SAFETY","CLA-VAL","RELIEF","12 MM","BRASS","8.8 KG/CM2","SPRING STL","NPT X FNPT","58 mm","N/S","PRESSURE, SPRING","4th stage safety assembly","N/A","50-04"]
["Drakensberg Pumped Storage Scheme",77202,"VALVE: TYPE: DISCHARGE; VALVE SIZE: 103.7 MM; DESIGN RATING: 0-250 DEG C; TEMPERATURE RATING: 0-250 DEG C; CONNECTION: COMPRESSION; OPERATED: PRESSURE; BODY MATERIAL: STL; TRIM: DISC STL; REFERENCE NO: HT303814; ASSEMBLY; 3RD STAGE","CLA-VAL","DISCHARGE","103.7 MM","STL","0-250 DEG C","DISC STL","COMPRESSION","N/S","N/S","PRESSURE","3rd stage discharge service","0-250 DEG C","HT303814"]
["Drakensberg Pumped Storage Scheme",77194,"PISTON: DIMENSIONS: DIA 180 X THK 30 MM; MATERIAL: STL; APPLICATION: VALVE; DRAWING NO: HT 404769 REV 1; REFERENCE NO: 20; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","CLA-VAL","PISTON","180 MM","STL","N/S","N/S","TBC","N/S","N/S","TBC","VALVE","N/S","20; HT 404769 REV 1"]
["Drakensberg Pumped Storage Scheme",77195,"VALVE, BALL: VALVE SIZE: 3 IN; DESIGN RATING: 150 LB; CONNECTION: FLANGE; BODY MATERIAL: STEEL; OPERATED: ACTUATOR; STYLE: BOLTED BONNET; TRIM: BALL STL; DRAWING NO: HT303978 REV 1; REFERENCE NO: 53-50; AG-13 TORQUE CYLINDER EQ 105","CLA-VAL","BALL","3 IN","STEEL","150 LB","BALL STL","FLANGE","N/S","N/S","ACTUATOR","Hydraulic oil / control fluid service","−29 °C to +200 °C","53-50; HT303978 REV 1"]
["Drakensberg Pumped Storage Scheme",77196,"CONNECTOR: TYPE: VALVE; DIMENSIONS: DIA (43-48) X LG 63 MM; MATERIAL: STL; DRAWING NO: HT 303978 REV 1; TORQUE CYLINDER","CLA-VAL","VALVE","34- 48 MM","STL","N/S","N/S","TBC","N/S","N/S","TBC","Hydraulic control fluid service","−20 °C to +80/100 °C","HT 303978 REV 1"]
["Drakensberg Pumped Storage Scheme",77200,"VALVE: TYPE: SUCTION; VALVE SIZE: 167 MM; CONNECTION: COMPRESSION; OPERATED: PRESSURE; BODY MATERIAL: STL; TRIM: DISC STL; REFERENCE NO: HT303809; 1ST STAGE","CLA-VAL","SUCTION","167 MM","STL","Ref. HT303809","DISC STL","COMPRESSION","7D size: 167 mm; connection: compression","N/S","PRESSURE","Compressed gas suction service","typically ~−20 °C to +60 °C suction conditions, up to ~120 °C depending on compressor design and OEM limits HT303809","HT303809"]
["Drakensberg Pumped Storage Scheme",77201,"VALVE: TYPE: DISCHARGE; VALVE SIZE: 145 MM; CONNECTION: COMPRESSION; OPERATED: PRESSURE; BODY MATERIAL: STL; TRIM: DISC STL; REFERENCE NO: HT303812; ASSEMBLY; 2ND STAGE","CLA-VAL","DISCHARGE","145 MM","STL","Ref. HT303812","DISC STL","COMPRESSION","7:ve size: 145 mm; connection: compression; operated: pressure","N/S","PRESSURE","Compressed gas discharge service","−20 °C to +160 °C","HT303812"]
["Drakensberg Pumped Storage Scheme",77203,"VALVE: TYPE: DISCHARGE; VALVE SIZE: 104.4 MM; CONNECTION: COMPRESSION; OPERATED: PRESSURE; BODY MATERIAL: STL; TRIM: DISC STL; REFERENCE NO: HT303816; ASSEMBLY; 4TH STAGE","CLA-VAL","DISCHARGE","104.4 MM","STL","Ref. HT303812","DISC STL","COMPRESSION","7Ive size: 104.4 mm; connection: compression; operated: pressure","N/S","PRESSURE","High-pressure compressed gas discharge service","N/A","HT303816"]
["Drakensberg Pumped Storage Scheme",77212,"VALVE, ANGLE: TYPE: NEEDLE; VALVE SIZE: 1/4 IN; CONNECTION: NPT; BODY MATERIAL: BRASS; OPERATED: HANDWHEEL; STYLE: THD BONNET; TRIM: STEM SS; REFERENCE NO: MB8-228.7553; T HANDLE","CLA-VAL","ANGLE; NEEDLE","1/4 IN","BRASS","Ref. No. MB8-228.7553","STEM SS","NPT","7: valve size: 1/4 in; connection: npt; body material: brass","N/S","HANDWHEEL","Instrumentation / control fluid service","−10 °C to +120 °C","MB8-228.7553"]
["Drakensberg Pumped Storage Scheme",77224,"VALVE, GATE: VALVE SIZE: 65 MM; CONNECTION: FLANGE; SLUICE 2-1/2 X 5K","KITZ Corporation","GATE","65 MM","STEAT",null,"N/S","FLANGE","N/S","N/S","Manual gate operation","Water service","~0 °C to +80 °C"]
["Drakensberg Pumped Storage Scheme",77226,"VALVE, GATE: VALVE SIZE: 50 MM; TYPE: SOLID WEDGE; CONNECTION: FNPT; BODY MATERIAL: BRASS; TRIM: DISC BRS; OPERATED: HANDWHEEL; STEM DESIGN: INSIDE SCREW; STYLE: 2 WAY; BONNET ROCK SEALED; DESIGN RATING: 10 BAR; REFERENCE NO: 2BX10K","KITZ Corporation","GATE; SOLID WEDGE","50 MM","BRASS","10 BAR","DISC BRS; INSIDE SCREW","FNPT","N/S","N/S","HANDWHEEL","General utility water service","−10 °C to +120 °C","2BX10K"]
["Drakensberg Pumped Storage Scheme",77215,"VALVE: TYPE: DISCHARGE; REFERENCE NO: HT303798; 32-00; 1ST STAGE; RETAINER ASSY","CLA-VAL","DISCHARGE","Not specified","STEYP","N/S","N/S","COMPRESSION","N/S","N/S","TBC","Compressed gas discharge service","N/S","HT303798"]
["Drakensberg Pumped Storage Scheme",77216,"VALVE: REFERENCE NO: 33-00; HT303856; 2ND STAGE SUCTION; RETAINER ASSY","CLA-VAL","Compressor valve component","Not specified","STEEF","N/S","N/S","COMPRESSION","N/S","N/S","TBC","Compressed gas suction service","N/S","33-00"]
["Drakensberg Pumped Storage Scheme",77227,"VALVE, GATE: VALVE SIZE: 1/2 IN; TYPE: SOLID WEDGE; CONNECTION: FNPT; BODY MATERIAL: BRASS; TRIM: DISC BRS; OPERATED: HANDWHEEL; STEM DESIGN: INSIDE SCREW; STYLE: THD BONNET; DESIGN RATING: 10 BAR","KITZ Corporation","GATE; SOLID WEDGE","1/2 IN","BRASS","10 BAR","DISC BRS; INSIDE SCREW","FNPT","N/S","N/S","HANDWHEEL","General utility service","N/S"]
["Drakensberg Pumped Storage Scheme",77228,"VALVE, GLOBE: VALVE SIZE: 15 MM; OPERATED: HANDWHEEL; CONNECTION: FLANGE; BODY MATERIAL: BRASS; TRIM: BONNET BRS; STEM DESIGN: INSIDE SCREW; STYLE: THD BONNET; DESIGN RATING: 10 BAR; 1/2BX10K","KITZ Corporation","GLOBE","15 MM","BRASS","10 BAR","BONNET BRS; INSIDE SCREW","FLANGE","N/S","N/S","HANDWHEEL","General utility water service","N/S"]
["Drakensberg Pumped Storage Scheme",77220,"VALVE, RELIEF: VALVE SIZE: 3/8 IN; SET PRESSURE: 1750 KPA; CONNECTION: BSP; BODY MATERIAL: BRASS; TRIM: SPRING STL; OPERATED: SPRING; AIR SAFETY","KITZ Corporation","RELIEF","3/8 IN","BRASS","1750 KPA","SPRING STL","BSP","95 in","N/S","SPRING","Compressed air / pneumatic safety relief service","N/S"]
["Drakensberg Pumped Storage Scheme",77221,"VALVE: TYPE: LOW PRESSURE; VALVE SIZE: 100.5 MM; CONNECTION: COMPRESSION; OPERATED: PRESSURE; BODY MATERIAL: STAINLESS STEEL; TRIM: DISC SS; REFERENCE NO: L.P.HTWT409571; L.P.; BA COMP 26/4","CLA-VAL","LOW PRESSURE","100.5 MM","STAINLESS STEEL","Ref. L.P.HTWT409571","DISC SS","COMPRESSION","7Nvalve size: 100.5 mm; connection: compression; operated: pressure","N/S","PRESSURE","Low-pressure compressed gas service","−20 °C to +120 °C","L.P.HTWT409571"]
["Drakensberg Pumped Storage Scheme",77229,"VALVE, GLOBE: VALVE SIZE: 20 MM; OPERATED: HANDWHEEL; CONNECTION: FLANGE; BODY MATERIAL: BRASS; TRIM: BONNET BRS; STEM DESIGN: INSIDE SCREW; STYLE: THD BONNET; DESIGN RATING: 150 LB; FIG NO: 1035","KITZ Corporation","GLOBE","20 MM","BRASS","150 LB","BONNET BRS; INSIDE SCREW","FLANGE","N/S","N/S","HANDWHEEL","General utility service","N/S",1035]
["Drakensberg Pumped Storage Scheme",77240,"VALVE, CHECK: TYPE: SWING; VALVE SIZE: 10 IN; DESIGN RATING: 10 BAR; CONNECTION: FLANGE; BODY MATERIAL: STEEL; STYLE: BOLTED CAP; TRIM: BONNET/DISC STL; REFERENCE NO: K2N078015","KITZ Corporation","CHECK; SWING","10 IN","STEEL","10 BAR","BONNET/DISC STL","FLANGE","7Yvalve size: 10 in; design rating: 10 bar","N/S","PRESSURE","Water / utility fluid service","N/S","K2N078015"]
["Drakensberg Pumped Storage Scheme",77231,"VALVE, GLOBE: VALVE SIZE: 40 MM; OPERATED: HANDWHEEL; CONNECTION: FLANGE; BODY MATERIAL: BRASS; TRIM: BONNET BRS; STEM DESIGN: INSIDE SCREW; STYLE: THD BONNET; DESIGN RATING: 5 BAR","KITZ Corporation","GLOBE","40 MM","BRASS","5 BAR","BONNET BRS; INSIDE SCREW","FLANGE","N/S","N/S","HANDWHEEL","Low-pressure utility water service","N/S"]
["Drakensberg Pumped Storage Scheme",77233,"VALVE, CHECK: VALVE SIZE: 50 MM; CONNECTION: FLANGE; BODY MATERIAL: CI; STYLE: BOLTED CAP; TRIM: DISC STL; REFERENCE NO: CRF15; K2N170038; TYPE LIFT; YUKEN RIGHT ANGLE","LIFT","CHECK","50 MM","CI","Ref. CRF15 / K2N170038","DISC STL","FLANGE","7N0 mm","N/S","PRESSURE","Hydraulic fluid service","N/S","CRF15"]
["Drakensberg Pumped Storage Scheme",77242,"VALVE, ANGLE: TYPE: GLOBE; VALVE SIZE: 100 MM; DESIGN RATING: 600 LB; CONNECTION: FLANGE; BODY MATERIAL: STL; OPERATED: HYDRAULIC; STYLE: BOLTED BONNET; TRIM: BONNET/STEM STL; DRAWING NO: M-6WO78AG8 REV 1; REFERENCE NO: 20DA1/2; AIR ADMISSION; FOR TAIL WATER DEPRESSING","CLA-VAL","ANGLE; GLOBE","100 MM","STL","600 LB","BONNET/STEM STL","FLANGE","95 mm","N/S","HYDRAULIC","Air admission service","N/S","20DA1/2; M-6WO78AG8 REV 1"]
["Drakensberg Pumped Storage Scheme",77243,"VALVE, GLOBE: VALVE SIZE: 38 MM; OPERATED: HANDWHEEL; CONNECTION: FNPT; BODY MATERIAL: STL; TRIM: BONNET STL; GRADE: 1.4021; STEM DESIGN: INSIDE SCREW; STYLE: THD BONNET; REFERENCE NO: 1-4021; NEEDLE; FOR HYDRAULIC STRUCTURES; SIZE 40MM","KITZ Corporation","GLOBE","38 MM","STL","Ref. 1-4021","BONNET STL; INSIDE SCREW","FNPT","7D8 mm","N/S","HANDWHEEL","Hydraulic water service","N/S","4021-01-01"]
["Drakensberg Pumped Storage Scheme",77236,"VALVE, GLOBE: VALVE SIZE: 2 IN; OPERATED: HANDWHEEL; CONNECTION: FLANGE; BODY MATERIAL: STL; TRIM: BONNET STL; STEM DESIGN: INSIDE SCREW; STYLE: BOLTED BONNET; REFERENCE NO: 790852-2","KITZ Corporation","GLOBE","2 IN","STL","Ref. No. 790852-2","BONNET STL; INSIDE SCREW","FLANGE","7E in","N/S","HANDWHEEL","General process / utility fluid service","N/S","790852-2"]
["Drakensberg Pumped Storage Scheme",77237,"VALVE, GATE: VALVE SIZE: 150 MM; TYPE: SOLID WEDGE; CONNECTION: FLANGE; BODY MATERIAL: CI; TRIM: BONNET/DISC CI; OPERATED: HANDWHEEL; STEM DESIGN: RISING OUTSIDE SCREW; STYLE: BOLTED BONNET; REFERENCE NO: 6BX10K","KITZ Corporation","GATE; SOLID WEDGE","150 MM","CI","JIS 10K","BONNET/DISC CI; RISING OUTSIDE SCREW","FLANGE","7O0 mm","N/S","HANDWHEEL","Water service","typically ~−10 °C to +120/150 °C for cast iron gate valves, depending on seat and gasket materials)","6BX10K"]
["Drakensberg Pumped Storage Scheme",77238,"VALVE, GATE: VALVE SIZE: 200 MM; TYPE: SOLID WEDGE; CONNECTION: FLANGE; BODY MATERIAL: STL; TRIM: BONNET STL; OPERATED: HANDWHEEL, GEAR; STEM DESIGN: RISING OUTSIDE SCREW; STYLE: BOLTED BONNET; REFERENCE NO: 8BX10K","KITZ Corporation","GATE; SOLID WEDGE","200 MM","STL","JIS 10K","BONNET STL; RISING OUTSIDE SCREW","FLANGE","7R0 mm","N/S","HANDWHEEL, GEAR","Water / utility water service","N/S","8BX10K"]
["Drakensberg Pumped Storage Scheme",77244,"VALVE, BALL: VALVE SIZE: 30 MM; DESIGN RATING: 315 BAR; CONNECTION: FNPT; BODY MATERIAL: STEEL; OPERATED: LEVER; STYLE: 2 WAY; TRIM: BALL SS; REFERENCE NO: KHR1; LINE MOUNTED; NW25; FOR HYDRAULIC STEEL STRUCTURES","HYDAC","BALL","30 MM","STEEL","315 BAR","BALL SS","FNPT","200 mm","N/S","LEVER","High-pressure hydraulic fluid service","Not specified (typically ~−20 °C to +80/100 °C for hydraulic 315 bar ball valves, depending on seal and seat materials)","KHR1"]
["Drakensberg Pumped Storage Scheme",77245,"VALVE, BALL: VALVE SIZE: 45 MM; DESIGN RATING: 200 BAR; CONNECTION: FNPT; BODY MATERIAL: STEEL; OPERATED: LEVER; STYLE: 2 WAY; TRIM: BALL STL; LINE MOUNTED; 1-1/2 IN (NW40); 8/81 Z","HYDAC","BALL","45 MM","STEEL","200 BAR","BALL STL","FNPT","200 mm","N/S","LEVER","High-pressure hydraulic fluid service","N/S"]
["Drakensberg Pumped Storage Scheme",77246,"VALVE, CHECK: TYPE: PISTON; VALVE SIZE: 3/4 IN; CONNECTION: FNPT; BODY MATERIAL: STL; STYLE: THD CAP; TRIM: DISC STL; REFERENCE NO: 1VR06R; LINE MOUNTED; FOR HYDRAULIC STEEL STRUCTURES","HYDAC","CHECK; PISTON","3/4 IN","STL","Ref. No. 1VR06R","DISC STL","FNPT","190 mm","N/S","PRESSURE, SPRING","Hydraulic fluid service","N/S","1VR06R"]
["Drakensberg Pumped Storage Scheme",77247,"VALVE, CHECK: TYPE: PISTON; VALVE SIZE: 1-1/2 IN; CONNECTION: FNPT; BODY MATERIAL: STL; STYLE: THD CAP; TRIM: DISC STL; REFERENCE NO: 1V12; LINE MOUNTED; FOR HYDRAULIC STEEL STRUCTURES","HYDAC","CHECK; PISTON","1-1/2 IN","STL","Ref. No. 1V12","DISC STL","FNPT","190 mm","N/S","PRESSURE, SPRING","Hydraulic fluid service","N/S","1V12"]
["Drakensberg Pumped Storage Scheme",77248,"VALVE, RELIEF: VALVE SIZE: 22 MM; BODY MATERIAL: STL; TRIM: SPRING STL; OPERATED: PRESSURE; ABEX DENISON FOR HYDRAULIC STEEL STRUCTURES; MANIFOLD","Parker Hannifin","RELIEF","22 MM","STL","N/S","SPRING STL","Manifold mounted","95 mm","N/S","PRESSURE","Hydraulic fluid pressure relief service","N/S"]
["Drakensberg Pumped Storage Scheme",77249,"VALVE: TYPE: FLOW CONTROL; VALVE SIZE: 27 MM; OPERATED: PRESSURE; BODY MATERIAL: CI; STYLE: 2 WAY; TRIM: BONNET CI; CONNECTION MANIFOLD; FOR HYDRAULIC STEEL STRUCTURES","Parker Hannifin","FLOW CONTROL","27 MM","CI","N/S","BONNET CI","Manifold mounted","95 mm","N/S","PRESSURE","Hydraulic fluid flow control service","N/S"]
["Drakensberg Pumped Storage Scheme",78752,"BELLOWS: TYPE: VALVE SAFETY RELIEF EMNIBC0080E; MATERIAL: SS Z6CNDT17-12; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Emerson Electric","VALVE SAFETY RELIEF EMNIBC0080E","80 MM","SS Z6CNDT17-12","N/S","N/S","TBC","N/S","N/S","PRESSURE","Safety relief valve pressure containment service","N/S"]
["Drakensberg Pumped Storage Scheme",85607,"BOLT: TYPE: VALVE; DIAMETER: 3/4 IN; LENGTH: 3-1/4 IN; HEAD: RD; MATERIAL: STL; THREAD: 16UNF; REFERENCE NO: 3W21453; FOR TYPE 30 MODEL 15T2 ING-RAND AIR COMPRESSOR","FOR TYPE 30; Ing-Rand","VALVE","3/4 IN","STL","Ref. 3W21453","N/S","THREAD:16 UNF","N/S","N/S","TBC","Compressed air service","N/S","3W21453"]
["Drakensberg Pumped Storage Scheme",85608,"BOLT: TYPE: VALVE; DIAMETER: 5/8 IN; LENGTH: 3 IN; HEAD: RD; MATERIAL: STL; THREAD: 18UNF; MODEL NO: 15T2; REFERENCE NO: 3W21454; TYPE 30","CLA-VAL","VALVE","5/8 IN","STL","Ref. 3W21454","N/S","THREAD:18 UNF","N/S","N/S","TBC","Compressed air service","N/S","3W21454; 15T2"]
["Drakensberg Pumped Storage Scheme",85609,"BOLT: TYPE: VALVE; DIAMETER: 5/8 IN; LENGTH: 2-5/8 IN; HEAD: RD; MATERIAL: STL; THREAD: 18UNF; REFERENCE NO: 3W21942; FOR TYPE 30 MODEL 15T2; ING-RAND COMPRESSOR","FOR TYPE 30; Ing-Rand","VALVE","5/8 IN","STL","Ref. 3W21454","N/S","THREAD:18 UNF","N/S","N/S","TBC","Compressed air service","−20 °C to +120 °C or up to ~400 °C","3W21942"]
["Drakensberg Pumped Storage Scheme",102600,"KIT: TYPE: OVERHAUL; APPLICATION: SAFETY VALVE; KIT CONSISTS: SPRING ITEM 46; PISTON ITEM 11; JOINT METAL O-RING ITEM 40XX2; JOINT METAL O-RING ITEM 43; SEAT ITEM 6; JOINT O-RING ITEM 89; SEAL ITEM 99","CLA-VAL","OVERHAUL","N/S","N/S","N/S","N/S","N/A","N/S","N/S","N/A","SAFETY VALVE","N/S",null,null,6]
["Drakensberg Pumped Storage Scheme",107087,"GASKET, PRE CUT: TYPE: VALVE CAGE CAP; REFERENCE NO: X1014T5; L.P, FOR TYPE 30 MODEL 41 ING-RAND COMPRESSOR 30550784","FOR TYPE 30; Ing-Rand","VALVE CAGE CAP","N/S","N/S","N/S","N/S","TBC","N/S","N/S","PRESSURE","Low-pressure compressed air service","−20 °C to +120 °C","X1014T5"]
["Drakensberg Pumped Storage Scheme",109457,"HANDLE: TYPE: VALVE; DIMENSIONS: LG 750 MM; MATERIAL: STL; REFERENCE NO: SW22; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","CLA-VAL","VALVE","750 MM","STL","N/S","N/S","TBC","N/S","N/S","HAND OPERATED","Manual valve operation accessory","N/S","SW22"]
["Drakensberg Pumped Storage Scheme",127130,"SOLENOID, ELECTRICAL: DUTY TYPE: VALVE; COIL VOLTAGE: 220 VAC; REFERENCE NO: 7601-0476; SOLENOIDS, 20 PU, 220V DC, 35VA","Parker Hannifin","VALVE","20 PU","N/S","N/S","N/S","TBC","N/S","N/S","SOLENOID","Valve actuation control service","N/S","7601-0476"]
["Drakensberg Pumped Storage Scheme",111786,"SPRING: TYPE: VALVE; DIMENSIONS: DIA 14 X LG 67 MM; MATERIAL: SPRING STL; MODEL NO: 41; REFERENCE NO: X1091PP 556; UNLOADER PLUNGER; FOR TYPE 30 AIR COMPRESSOR","CLA-VAL","VALVE","14 mm","SPRING STL","Ref. X1091PP 556","N/S","TBC","N/S","N/S","SPRING","Compressed air service","N/S","X1091PP 556; 41"]
["Drakensberg Pumped Storage Scheme",111801,"SPRING: TYPE: VALVE; DIMENSIONS: DIA (6 X 6.6) X LG 14.7 X THK 1 MM; MATERIAL: SPRING STL; REFERENCE NO: HT403875; FOR PLATE; 2ND, 3RD, 4TH STAGE; STAINLESS STEEL WIRE","CLA-VAL","VALVE","6 MM","SPRING STL","Ref. HT403875","N/S",null,"N/S","N/S","SPRING","Compressed gas service","N/S","HT403875"]
["Drakensberg Pumped Storage Scheme",111803,"SPRING: TYPE: VALVE; DIMENSIONS: DIA (6.5 X 7) X LG 11.8 X THK 1 MM; MATERIAL: SPRING STL; REFERENCE NO: HT403877; FOR BACKING PLATE; 2ND,3RD,4TH STAGE; STAINLESS STEEL WIRE","CLA-VAL","VALVE","7 mm OD × 11.8 mm Length × 1.0 mm Wire Diameter","SPRING STL","Ref. HT403877","N/S",null,"801 dia","N/S","SPRING","Compressed gas service","N/S","HT403877"]
["Drakensberg Pumped Storage Scheme",128439,"SOLENOID, ELECTRICAL: DUTY TYPE: VALVE; COIL VOLTAGE: 24 VDC; REFERENCE NO: GS 40-4N-B; SINGLE DIRECT CONTROL, 100 PCTED, 0.79A, 3-13533-41, 21/80, HYDRONORMA","Hydronorma","VALVE","GS 40","STEEL","N/S","N/S",null,"N/S","N/S","SOLENOID","Hydraulic fluid control service","N/S","GS 40-4N-B"]
["Drakensberg Pumped Storage Scheme",123504,"VALVE, SOLENOID: PIPE SIZE: 8 MM; STYLE: 3 WAY; POTENTIAL: 24 VDC; BODY MATERIAL: STEEL; MEDIUM: OIL; CURRENT: 0.79 A; CONNECTION MANIFOLD; GENERAL PURPOSE ENCLOSURE; CONTROL","Hydronorma","SOLENOID","8 MM","STEEL","N/S","N/S","Manifold mounted","N/S","N/S","SOLENOID","OIL","N/S",null,"24 VDC; 0.79 A"]
["Drakensberg Pumped Storage Scheme",125604,"SOLENOID, ELECTRICAL: DUTY TYPE: VALVE; COIL VOLTAGE: 220 VAC; REFERENCE NO: 331B21; LUCIFER, 15 BAR, 3 WAY","Lucifer SA","VALVE","1/2 inch","typically brass","15 BAR","N/S","TBC","N/S","N/S","SOLENOID","Pneumatic / fluid control service","N/S","331B21"]
["Drakensberg Pumped Storage Scheme",126169,"SOLENOID, ELECTRICAL: DUTY TYPE: AIR VALVE; COIL VOLTAGE: 220 VAC; SUPPL P/N: FF32-35; 617194; REFERENCE NO: PN 617194; 617194; FOR AIR VALVE FF32/35, 50 HZ, 100PCT ED, IP65, ASH HANDLING PLANT EQUIPMENT INCLUDING LIFTING DEVICE AND IMMERSION DAMPERS FF31/35, 55 VA","Parker Hannifin","AIR VALVE","TBC","TBC","100% ED/220 VAC, 50 Hz, 55 VA","N/S","TBC","N/S","N/S","SOLENOID","Compressed air / pneumatic control service","N/S","FF32-35; PN 617194"]
["Drakensberg Pumped Storage Scheme",177811,"VALVE, ANGLE: TYPE: GLOBE; VALVE SIZE: 150 MM; DESIGN RATING: 150 LB; CONNECTION: FLANGE; BODY MATERIAL: STL; OPERATED: HYDRAULIC; STYLE: BOLTED BONNET; TRIM: SEAT HF; GRADE: SCPH2; AIR EXHAUST; AUTOMATIC; FOR DEWATERING AIR EXHAUST PIPE LINE","CLA-VAL","ANGLE; GLOBE","150 MM","STL","150 LB","SEAT HF","FLANGE","N/S","N/S","HYDRAULIC","Air exhaust / venting service","N/S",null,null,"F"]
["Drakensberg Pumped Storage Scheme",502387,"VALVE: TYPE: COMPRESSOR 3RD STAGE; OPERATED: AUTOMATIC; BODY MATERIAL: STL; SUPPL P/N: 31517725","Atlas Copco","COMPRESSOR 3RD STAGE","20 GA","STL","N/S","N/S","COMPRESSION","N/S","N/S","AUTOMATIC","Compressed air service","N/S",31517725]
["Drakensberg Pumped Storage Scheme",178035,"VALVE, RELIEF: REFERENCE NO: 0523C","KITZ Corporation","RELIEF","1/2 IN AND 3/4 IN","STEEL","N/S","N/S","TBC","N/S","N/S","PRESSURE","Pressure relief / safety protection service","N/S","0523C"]
["Drakensberg Pumped Storage Scheme",178037,"VALVE, GATE: VALVE SIZE: 4 IN; DRAWING NO: MB9-341.3200B REV 1; RELAY; ASSEMBLY 4","KITZ Corporation","GATE","4 IN","STEAT","N/S","N/S","TBC","N/S","N/S","TBC","Industrial utility/process service","N/S","MB9-341.3200B REV 1"]
["Drakensberg Pumped Storage Scheme",502388,"VALVE: TYPE: COMPRESSOR 2ND STAGE; OPERATED: AUTOMATIC; BODY MATERIAL: STL; SUPPL P/N: 37004827","Atlas Copco","COMPRESSOR 2ND STAGE","35 GA","STL","N/S","N/S","COMPRESSION","N/S","N/S","AUTOMATIC","Compressed air service","N/S",37004827]
["Drakensberg Pumped Storage Scheme",178437,"VALVE, NEEDLE: VALVE SIZE: 6 IN; CONNECTION: FLANGE; BODY MATERIAL: STL","KITZ Corporation/Velan","NEEDLE","6 IN","STL","N/S","N/S","FLANGE","95 in","N/S","Manual valve operation","Process / utility fluid control service","N/S"]
["Drakensberg Pumped Storage Scheme",178522,"VALVE, ANGLE: TYPE: PLUG; VALVE SIZE: 100 MM; CONNECTION: FLANGE; BODY MATERIAL: CI; OPERATED: HYDRAULIC; STYLE: BOLTED BONNET; TRIM: DISC STL","CLA-VAL","ANGLE; PLUG","100 MM","CI","N/S","DISC STL","FLANGE","8Balve size: 100 mm","N/S","HYDRAULIC","Water service","N/S"]
["Drakensberg Pumped Storage Scheme",178523,"VALVE, ANGLE: TYPE: PLUG; VALVE SIZE: 250 MM; CONNECTION: FLANGE; BODY MATERIAL: STL; OPERATED: HYDRAULIC; STYLE: BOLTED BONNET; TRIM: DISC STL","Howell-Bunger Valves","ANGLE; PLUG","250 MM","STL","N/S","DISC STL","FLANGE","8 alve size: 250 mm","N/S","HYDRAULIC","Water service","N/S"]
["Drakensberg Pumped Storage Scheme",205470,"KIT: TYPE: SEALS; APPLICATION: SPH/VALVE OPERATOR; COMPRISING: ROOF TYPE LIP RING; SUPPORTING RING; THRUST RING; REFERENCE NO: 1162-015.532; 1160-014.832; 1161-015.229; CONSISTS OF ON3 OF 3; SIZE ID 250 X OD 280 MM","LIP","SEALS","N/A","N/A","Ref. Nos. 1162-015.532 / 1160-014.832 / 1161-015.229","N/S","N/A","N/S","N/S","N/A","SPH/VALVE OPERATOR","N/S","1162-015.532"]
["Drakensberg Pumped Storage Scheme",401291,"VALVE, BALL: VALVE SIZE: 3/4 IN; OPERATED: HANDLE; TYPE: STOP","KITZ Corporation/Apollo Valves","BALL; STOP","3/4 IN","STEAL","N/S","N/S","TBC","95 in","N/S","HANDLE","Isolation service","N/S"]
["Drakensberg Pumped Storage Scheme",502390,"VALVE: CONNECTION: COMPRESSION; OPERATED: AUTOMATIC; BODY MATERIAL: STEEL; TRIM: DISC STL; SOFTGOODS: GASKET; MANUF P/N: 32134058","Atlas Copco","Automatic valve",null,"STEEL","N/S","DISC STL","COMPRESSION","N/S","N/S","AUTOMATIC","Compressor service","N/S",32134058,null,"GASKET"]
["Drakensberg Pumped Storage Scheme",502396,"VALVE: TYPE: 1ST STAGE; VALVE SIZE: 164MM X 85 IN; TEMPERATURE RATING: 0-250 DEG C; CONNECTION: COMPRESSION; OPERATED: AUTOMATIC; BODY MATERIAL: STEEL; MANUF P/N: 37101946","Atlas Copco","1ST STAGE","164MM X 85 IN","STEEL","N/S","N/S","COMPRESSION","2Ave size: 164mm x 85 in","N/S","AUTOMATIC","Compressed air / process gas service","0-250 DEG C",37101946]
["Drakensberg Pumped Storage Scheme",594825,"KIT: TYPE: REPAIR T125; APPLICATION: PRESSURE RELIEF VALVE","Tyco Valves & Controls","REPAIR T125","N/A","N/A","N/S","N/S","N/A","N/S","N/S","N/A","PRESSURE RELIEF VALVE","N/S"]
["Drakensberg Pumped Storage Scheme",621290,"KIT, VALVE REPAIR: TYPE: BALL VALVE 1/2 IN; APPLICATION: VALVE INTERNAL; SPECIFICATION: B16; COMPRISING: BODY SEAL; SEALS; STEM BEARING; STEM PACKING; SUPPL P/N: 23804289","Atlas Copco","BALL VALVE 1/2 IN","N/A","N/A","N/S","N/S","N/A","N/S","N/S","N/A","VALVE INTERNAL","depends on valve and seal materials; typically −20 °C to +100 °C or up to ~200 °C depending on sealing compound type",23804289]
["Drakensberg Pumped Storage Scheme",621484,"VALVE, BUTTERFLY: TYPE: LUG WAFER; VALVE SIZE: 150 MM; DESIGN RATING: PN16; TEMPERATURE RATING: 0-120 DEG C; CONNECTION: LUG; BODY MATERIAL: DI; FACE TO FACE LENGTH: 59 MM; OPERATED: ACTUATOR; TRIM: RUBBER LINED; SOFTGOODS: SEAL; APPLICATION: TURBINE PROTECTION; GRADE: GGG40; SHAFT CONNECTION: DIA 14MM","KSB","BUTTERFLY; LUG WAFER","150 MM","DI","PN16","RUBBER LINED","LUG; DIA 14MM","59 MM","N/S","ACTUATOR","TURBINE PROTECTION","0-120 DEG C",null,null,"SEAL"]
["Drakensberg Pumped Storage Scheme",628662,"VALVE: TYPE: SAFETY; VALVE SIZE: 4 IN; DESIGN RATING: 53 BAR; TEMPERATURE RATING: 538 DEG C; CONNECTION: FLANGE; OPERATED: PRESSURE, SPRING, 0-35 LB; BODY MATERIAL: BS 1504-240; STYLE: ANGLE PATTERN; TRIM: PT; OEM P/N: 4\"707 SD; DRAWING NO: F5217/5 REV 0; .","Crosby Valve","SAFETY","4 IN","BS 1504-240","53 BAR","PT","FLANGE","95 in","N/S","PRESSURE, SPRING, 0-35 LB","High-temperature pressure relief service","538 DEG C","4\"707 SD; F5217/5 REV 0"]
["Drakensberg Pumped Storage Scheme",637382,"VALVE: TYPE: CONCENTRIC; VALVE SIZE: OD 225 X THK 30 MM; DESIGN RATING: 380 BAR; TEMPERATURE RATING: -28 TO 425 DEG C; CONNECTION: SEAT; OPERATED: MECHANICAL; BODY MATERIAL: STAINLESS STEEL; STYLE: LEAF; MANUF P/N: 37134; MODEL NO: WP6310; FOR USE ON JP SAUER AND SOHN COMPRESSOR","J.P. Sauer & Sohn Maschinenbau GmbH","CONCENTRIC","OD 225 X THK 30 MM","STAINLESS STEEL","380 BAR","N/S","SEAT","95 mm","N/S","MECHANICAL","JP SAUER AND SOHN COMPRESSOR","-28 TO 425 DEG C","37134; WP6310"]
["Drakensberg Pumped Storage Scheme",640478,"VALVE, GLOBE: VALVE SIZE: 2 IN; DESIGN PRESSURE: 102 BAR; DESIGN TEMPERATURE: -29 TO 38 DEG C; FACE TO FACE LENGTH: 292.1 MM; OPERATED: HANDWHEEL, MANUAL; CONNECTION: FLANGE; BODY MATERIAL: A216 GR WCB; TRIM: A182F6; GRADE: A216 GR WCB; SOFTGOODS: PACKING GRAPHITE; STEM DESIGN: A182F6; APPLICATION: RUNNER SEAL ISOLATION; SPECIFICATION: CL 600; TYPE: ISOLATING; DESIGN RATING: ASME B19.34; TEMPERATURE RATING: ASME B16.34; CONNECTION ASME B16.5/B16.25; TESTING AND INSPECTION; API 598","Flowserve","GLOBE; ISOLATING","2 IN","A216 GR WCB","ASME B19.34; 102 BAR","A182F6","FLANGE","292.1 MM","N/S","HANDWHEEL, MANUAL","RUNNER SEAL ISOLATION","ASME B16.34; -29 TO 38 DEG C",null,null,"PACKING GRAPHITE"]
["Drakensberg Pumped Storage Scheme",640479,"VALVE, BUTTERFLY: TYPE: DRAIN WAFER; VALVE SIZE: DN 32; DESIGN RATING: PN25; TEMPERATURE RATING: NBR -10 TO 90 DEG C; CONNECTION: FLANGE; BODY MATERIAL: 2EN-GJS-4000-15(GGG-40) EPOXY COATED 120 UM; FACE TO FACE LENGTH: 33 MM; OPERATED: ACTUATOR PNEUMATIC; TRIM: A1.4408 INVESTMENT CASTING; SOFTGOODS: NBR; APPLICATION: SHAFT/RUNNER SEAL DRAIN; GRADE: DN 25-600; SPECIFICATION: D480; SCHEDULE: ASME B16.47; SERIES A; CL 150; SPECIAL FEATURES: BARE SHAFT; SUPPL P/N: D480 32W332A1NLF07 D11; CONNECTION TYPE; 3EN1092 PN16, OPERATING PRESSUE; 3.16 BAR, SHAFT MATERIAL; 1AISI420/1.4021, SHAFT LENGTH; 18, 18 MM, SEAT LINER; N NBR","KSB","BUTTERFLY; DRAIN WAFER","DN 32","2EN-GJS-4000-15(GGG-40) EPOXY COATED 120 UM","PN25","A1.4408 INVESTMENT CASTING","FLANGE","33 MM","N/S","ACTUATOR PNEUMATIC","SHAFT/RUNNER SEAL DRAIN","NBR -10 TO 90 DEG C","D480 32W332A1NLF07 D11",null,"NBR; R"]
["Drakensberg Pumped Storage Scheme",647409,"VALVE, SOLENOID: PIPE SIZE: 6 X 4 MM; STYLE: 3/2 WAY; POTENTIAL: 230 VAC; DESIGN RATING: 0-10 BAR; CONNECTION: G1/8 IN-BSPP; BODY MATERIAL: BRASS; OPERATED: AIR; ENCLOSURE RATING: IP65; MEDIUM: NATURAL GASES; FLUIDS; POWER: 8 W; ORIFICE SIZE: 2 MM; COIL: POLYAMIDE; SOFTGOODS: FKM; APPLICATION: FIRE DAMPER","ASCO","SOLENOID","6 X 4 MM; 2 MM","BRASS","0-10 BAR","N/S","G1/8 IN-BSPP","95 mm","N/S","AIR","NATURAL GASES; FIRE DAMPER","−20 °C to +90 °C",null,"230 VAC; 8 W; POLYAMIDE; IP65","FKM"]
["Drakensberg Pumped Storage Scheme",654743,"VALVE, BALL: VALVE SIZE: 1/2 IN; APPLICATION: AMMONIA SOLUTION LINE TO FEEDWATER TANK; TYPE: QUICK STOP; SUPPL P/N: N300","Spirax Sarco","BALL; QUICK STOP","1/2 IN","STEEL","N/S","N/S","TBC","N/S","N/S","Manual shut-off service","AMMONIA SOLUTION LINE TO FEEDWATER TANK","20–60 °C","N300"]
["Drakensberg Pumped Storage Scheme",655344,"CONE: TYPE: SHUT-OFF VALVE; SUPPL P/N: SP-KUS-F2-16433; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","KSB","SHUT-OFF VALVE",null,"STPE","N/S","N/S","TBC","N/S","N/S","TBC","Valve shut-off service","N/S","SP-KUS-F2-16433"]
["Drakensberg Pumped Storage Scheme",662034,"VALVE, RELIEF: VALVE SIZE: 20 MM; SET PRESSURE: 7000 KPA; TEMPERATURE RATING: -25 TO 400 DEG C; CONNECTION: HEX NIPPLE 20 MM; BODY MATERIAL: BRONZE; TRIM: CRNI STEEL BRONZE; FACE TO FACE LENGTH: S1=36; S2=44 MM; OPERATED: SPRING; SPECIFICATION: DIN 3230; APPLICATION: SV AIR MAKE-UP VESSEL; PRESSURE RANGE: 0-90 BAR; SPHERICAL VALVE AIR MAKE-UP VESSEL SAFETY VALVE","Bopp & Reuther Sicherheits- und Regelarmaturen GmbH","RELIEF","20 MM","BRONZE","0-90 BAR; 7000 KPA","CRNI STEEL BRONZE","HEX NIPPLE 20 MM","S1=36","N/S","SPRING","SV AIR MAKE-UP VESSEL","-25 TO 400 DEG C"]
["Drakensberg Pumped Storage Scheme",662552,"VALVE, CHECK: TYPE: NON RETURN; VALVE SIZE: 80 MM; DESIGN RATING: PN40; TEMPERATURE RATING: 50 DEG C; CONNECTION: BW; BODY MATERIAL: CI; FACE TO FACE LENGTH: 173 MM; OPERATED: AUTOMATIC; TRIM: STL; APPLICATION: LIMESTONE HYDRAULIC FEEDER DRIVE; SPECIFICATION: TH-CD-2572-00-02; SUPPL P/N: 2572-00-02-14","KSB","CHECK; NON RETURN","80 MM","CI","PN40","STL","BW","173 MM","N/S","AUTOMATIC","LIMESTONE HYDRAULIC FEEDER DRIVE","50 DEG C","2572-00-02-14"]
["Drakensberg Pumped Storage Scheme",662572,"VALVE, CHECK: TYPE: NON RETURN; VALVE SIZE: 100 MM; DESIGN RATING: PN25; TEMPERATURE RATING: 55 DEG C; CONNECTION: BW; BODY MATERIAL: CAST STL; FACE TO FACE LENGTH: 170 MM; OPERATED: FLOW; TRIM: STL; APPLICATION: LIMESTONE HYDRAULIC FEEDER DRIVE; SPECIFICATION: TH-CD-2572-00-02; SUPPL P/N: 2572-00-02-25","KSB","CHECK; NON RETURN","100 MM","CAST STL","PN25","STL","BW","170 MM","N/S","FLOW","LIMESTONE HYDRAULIC FEEDER DRIVE","55 DEG C","2572-00-02-25"]
["Drakensberg Pumped Storage Scheme",688832,"VALVE, RELIEF: VALVE SIZE: 1/2 X 3/4 IN; SET PRESSURE: 1100 KPA; TEMPERATURE RATING: -10 TO 300 DEG C; CONNECTION: MALE 0.5 IN; BODY MATERIAL: BRASS; TRIM: BRASS; FACE TO FACE LENGTH: 50X35 MM; OPERATED: LEVER; APPLICATION: COMPRESSOR; DESIGN RATING: 4314.93 KPA; TEST CERTIFICATE REQUIRED","BSP Valve","RELIEF","1/2 X 3/4 IN","BRASS","4314.93 KPA; 1100 KPA","BRASS","MALE 0.5 IN","50X35 MM","N/S","LEVER","Compressor","-10 TO 300 DEG C",{"$nulls":3},"CERTIFICATE REQUIRED"]
["Drakensberg Pumped Storage Scheme",696638,"VALVE, BUTTERFLY: TYPE: CENTERED DISC; VALVE SIZE: 3 IN; DESIGN RATING: PN35; TEMPERATURE RATING: 0-100 DEG C; CONNECTION: BW; BODY MATERIAL: 1.4571; FACE TO FACE LENGTH: 400 MM; OPERATED: MANUAL; TRIM: STL; SOFTGOODS: GASKETS; APPLICATION: DRAIN VALVE 1 TURBINE HOUSE UNIT 4; 4 0LCE10 AA401; SPECIFICATION: AV-25-63-SE-HR-G-XX-00; SUPPL P/N: 63906F3C7C3F09C3E0401EAC37FA0A05","KSB","BUTTERFLY; CENTERED DISC","3 IN",1.4571,"PN35","STL","BW","400 MM","N/S","MANUAL","DRAIN VALVE 1 TURBINE HOUSE UNIT 4","0-100 DEG C","63906F3C7C3F09C3E0401EAC37FA0A05",null,"GASKETS"]
["Drakensberg Pumped Storage Scheme",708296,"VALVE: TYPE: BYPASS; VALVE SIZE: 450 X 350 MM; DESIGN RATING: 7.2 MPA; TEMPERATURE RATING: 50 DEG C; FACE TO FACE LENGTH: 1070 MM; CONNECTION: 3/4 IN-BSP; OPERATED: HYDRAULIC; BODY MATERIAL: STAINLESS STEEL; STYLE: CYLINDRICAL; SOFTGOODS: O RINGS/GASKETS; OEM P/N: 891215705","KSB","BYPASS","450 X 350 MM","STAINLESS STEEL","7.2 MPA","N/S","3/4 IN-BSP","1070 MM","N/S","HYDRAULIC","Hydraulic water service","50 DEG C",891215705,null,"O RINGS/GASKETS"]
["Drakensberg Pumped Storage Scheme",715945,"VALVE, CHECK: TYPE: NON-RETURN; VALVE SIZE: 650 MM; DESIGN RATING: Y 0.35 AND VACUUM MPA; TEMPERATURE RATING: 200 DEG C; CONNECTION: BUTT-WELDED; BODY MATERIAL: STEEL ASTM A216-WCB; FACE TO FACE LENGTH: 1448 MM; OPERATED: AUTO; TRIM: STEEL; APPLICATION: CHECK VALVE LBS30AA501; SPECIFICATION: ANSI B16 34 CLASS 150; DRAWING NO: FB21EV650NFDA ITEM DEWRANCE; BLED STEAM CHECK VALVE, BODY: WBC, SEAT: CR13, DISK: CR18","Dewrance","CHECK; BODY; NON-RETURN","650 MM","STEEL ASTM A216-WCB","Y 0.35 AND VACUUM MPA","STEEL","BUTT-WELDED","1448 MM","N/S","AUTO","CHECK VALVE LBS30AA501","200 DEG C","FB21EV650NFDA ITEM DEWRANCE",null,"CR13, DISK: CR18"]
["Drakensberg Pumped Storage Scheme",738160,"VALVE: TYPE: NRV NON RETURN; VALVE SIZE: 1/2 IN; DESIGN RATING: 16 BAR; TEMPERATURE RATING: -198 TO 260 DEG C; CONNECTION: 1/2 IN; OPERATED: FLOW; BODY MATERIAL: STAINLESS STEEL 316; STYLE: 1 WAY; SOFTGOODS: GASKET; MANUF P/N: 111929400252002+00; REFERENCE NO: FTTPDS48E 01; SERGI FRANCE","SERGI France","NRV NON RETURN","1/2 IN","STAINLESS STEEL 316","16 BAR","N/S","1/2 IN","81 s, Face-to-Face, Drilling / PCD, Mediums, Face-to-Face, Drilling / PCD, Medium","N/S","FLOW","Process fluid / gas non-return service","-198 TO 260 DEG C","111929400252002+00; FTTPDS48E 01",null,"GASKET"]
["Drakensberg Pumped Storage Scheme",738822,"VALVE: TYPE: INJECTION; VALVE SIZE: 6/4 - R 1/2 IN; DESIGN RATING: 7-16 BAR; TEMPERATURE RATING: 25-40 DEG; CONNECTION: 6 MM COMPRESSION; OPERATED: STANDARD; BODY MATERIAL: PVC; .","Injection Valve / Dosing Valve","INJECTION","6/4 - R 1/2 IN","PVC","7-16 BAR","N/S","6 MM COMPRESSION","INJECTION; VALVE SIZE: 6/4 - R 104 s, Face-to-Face, Drilling / PCD, Mediums, Face-to-Face, Drilling / PCD, Medium","N/S","STANDARD","Chemical dosing / injection service","25-40 DEG"]
["Drakensberg Pumped Storage Scheme",738824,"VALVE: TYPE: FOOT; VALVE SIZE: 20 MM; DESIGN RATING: 7-16 BAR; TEMPERATURE RATING: 40 DEG; CONNECTION: 6 MM COMPRESSION; OPERATED: STANDARD; BODY MATERIAL: PVDF PTFE","Serto","FOOT","20 MM","PVDF PTFE","7-16 BAR","N/S","6 MM COMPRESSION","FOOT; VALVE SIZE: 2001 s, Face-to-Face, Drilling / PCD, Mediums, Face-to-Face, Drilling / PCD, Medium","N/S","STANDARD","Chemical dosing / suction foot valve service","40 DEG"]
["Drakensberg Pumped Storage Scheme",738906,"KIT, COMPRESSOR REPAIR: TYPE: SERVICE; APPLICATION: SPHERICAL VALVE; SPECIFICATION: ELECTRIC; COMPRISING: PISTON RINGS & GASKETS; MANUF P/N: 32226342; TYPE 30 MODEL 15T2, COMPRESSION STAGES 1, 2 AND 3, INGERSOLL RAND","TYPE 30; Ingersoll Rand","SERVICE","N/A","N/A","N/S","N/S","N/A","N/S","N/S","N/A","SPHERICAL VALVE","N/S",32226342]
["Ankerlig Power Station",74956,"VALVE, BALL: VALVE SIZE: 1-1/2 IN; DESIGN RATING: 600 LB; CONNECTION: BSP; BODY MATERIAL: CS; OPERATED: MANUAL; STYLE: 2 WAY; TRIM: BALL/STEM SS GR 304; SEAT PTFE",null,"BALL","1-1/2 IN","CS","600 LB","BALL/STEM SS GR 304","BSP",null,null,"MANUAL",{"$nulls":4},"E"]
["Ankerlig Power Station",233792,"VALVE, SOLENOID: PIPE SIZE: DN15; STYLE: 2 WAY; POTENTIAL: 220 VDC; DESIGN RATING: 100 BAR; CONNECTION: FLANGE; BODY MATERIAL: GR 1.4404/1.4571; OPERATED: NO; ENCLOSURE RATING: IP65; MEDIUM: HEIZOL; CURRENT: 0.22 A; ORIFICE SIZE: DN 15; COIL: 220 V DC; MANUF P/N: FK15NO1E; SUPPL P/N: A2A50187268; REFERENCE NO: PB0000144283; 503443; 2.5 M3/HR; WITH 4 X 14 MM DIA HOLES DRILLED INTO FLANGE","Muller Coax","SOLENOID","DN15; DN 15","GR 1.4404/1.4571","100 BAR",null,"FLANGE",null,null,"NO","HEIZOL",null,"FK15NO1E; A2A50187268; PB0000144283","220 VDC; 0.22 A; 220 V DC; IP65"]
["Ankerlig Power Station",233844,"VALVE, CHECK: BODY MATERIAL: CI; SUPPL P/N: MBV30AA201; C5V08311B5; LIFTING OIL; KKS; FOR USE ON LIFTING OIL PUMP MBV BASE PIPING ON GT AUX SYSTEM","Parker","CHECK",null,"CI",{"$nulls":6},"LIFTING OIL PUMP MBV BASE PIPING ON GT AUX SYSTEM",null,"MBV30AA201"]
["Ankerlig Power Station",233849,"VALVE, BALL: VALVE SIZE: 1 IN; DESIGN RATING: 40 BAR; CONNECTION: BSP; BODY MATERIAL: STAINLESS STEEL; OPERATED: LEVER; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: PTFE; SUPPL P/N: MBV23AA412; REFERENCE NO: SLV3800141; MBV25AA401; WITH ATTACHMENT, KKS; FOR USE ON LUBE OIL FILTER ON MBV BASE PIPING ON GT AUX SYSTEM",null,"BALL","1 IN","STAINLESS STEEL","40 BAR","STAINLESS STEEL","BSP",null,null,"LEVER","LUBE OIL FILTER ON MBV BASE PIPING ON GT AUX SYSTEM",null,"MBV23AA412; SLV3800141",null,"PTFE"]
["Ankerlig Power Station",233850,"VALVE: TYPE: ISOLATING; VALVE SIZE: NB 4; DESIGN RATING: 400 BAR; CONNECTION: BSP; OPERATED: HANDWHEEL; BODY MATERIAL: 1.046; STYLE: ISOLATE/VENT; REFERENCE NO: MBV31AA301; MBV31AA305; MBV21AA301; MBV23AA301; FOR USE ON GT AUX SYSTEMS",null,"ISOLATING","NB 4",1.046,"400 BAR",null,"BSP",null,null,"HANDWHEEL","GT AUX SYSTEMS",null,"MBV31AA301"]
["Ankerlig Power Station",233851,"VALVE: TYPE: BALANCE; VALVE SIZE: 3/8 IN; DESIGN RATING: 16 BAR; TEMPERATURE RATING: 80-100 DEG C; CONNECTION: 3/8 IN-BSPP; OPERATED: KNOB; BODY MATERIAL: STL HARDENED BS 970; SPECIFICATION: 305000; SPECIAL FEATURES: HAND WHEEL; STL VERSION; MANUF P/N: 305000; REFERENCE NO: SLV3800141; MBV25AA252; FOR USE ON LUBE OIL FILTER ON MBV BASE PIPING ON GT AUX SYSTEM",null,"BALANCE","3/8 IN","STL HARDENED BS 970","16 BAR",null,"3/8 IN-BSPP",null,null,"KNOB","LUBE OIL FILTER ON MBV BASE PIPING ON GT AUX SYSTEM","80-100 DEG C","305000; SLV3800141"]
["Ankerlig Power Station",233857,"VALVE, BUTTERFLY: TYPE: WAFER; VALVE SIZE: 150 MM; DESIGN RATING: PN16; TEMPERATURE RATING: -10 TO 80 DEG C; CONNECTION: FLANGE; BODY MATERIAL: STEEL; OPERATED: HANDLEVER; TRIM: STAINLESS STEEL; SOFTGOODS: RUBBER; REFERENCE NO: MBV21AA254; ECLS 71391; FOR USE ON MBV BASE PIPING ON GT AUX SYSTEM",null,"BUTTERFLY; WAFER","150 MM","STEEL","PN16","STAINLESS STEEL","FLANGE",null,null,"HANDLEVER","MBV BASE PIPING ON GT AUX SYSTEM","-10 TO 80 DEG C","MBV21AA254",null,"RUBBER"]
["Ankerlig Power Station",233859,"VALVE: TYPE: THROTTLE; CONNECTION: BOLTED; OPERATED: SCREW DOWN; BODY MATERIAL: STL; STYLE: 1 WAY; TRIM: STL; REFERENCE NO: MBV22AA281; FOR MBV BASE PIPING ON GT AUX SYSTEM",null,"THROTTLE",null,"STL",null,"STL","BOLTED",null,null,"SCREW DOWN",null,null,"MBV22AA281"]
["Ankerlig Power Station",233871,"VALVE, RELIEF: BODY MATERIAL: CAST IRON; DESIGN RATING: 210 BAR; SUPPL P/N: MBA30AA191; R5V 08 593 32 A5 152 210; REFERENCE NO: SLV 3720522; PARKER; KKS: FOR LIFTING OIL PUMP ON GT AUX SYSTEM","Parker","RELIEF",null,"CAST IRON","210 BAR",{"$nulls":7},"MBA30AA191; SLV 3720522"]
["Ankerlig Power Station",233872,"VALVE, RELIEF: BODY MATERIAL: CI; SUPPL P/N: R4V06 535 30 A5; MBV31AA151; REFERENCE NO: SLV3860114; PARKER, KKS; FOR CONTROL BLOCK LIFTING OIL ON MBV BASE PIPING ON GT AUX SYSTEM","Parker","RELIEF",null,"CI",{"$nulls":8},"R4V06 535 30 A5; SLV3860114"]
["Ankerlig Power Station",233891,"VALVE, BALL: VALVE SIZE: 1/4 IN; DESIGN RATING: 65; CONNECTION: THD; BODY MATERIAL: STAINLESS STEEL; OPERATED: LEVER; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: TEFLON; SUPPL P/N: MBV50AA503; KKS; USED ON MBV BASE PIPING ON GT AUX SYSTEMS",null,"BALL","1/4 IN","STAINLESS STEEL",65,"STAINLESS STEEL","THD",null,null,"LEVER","MBV BASE PIPING ON GT AUX SYSTEMS",null,"MBV50AA503",null,"TEFLON"]
["Ankerlig Power Station",233892,"VALVE, BALL: VALVE SIZE: 1/2 IN; DESIGN RATING: 65 BAR; CONNECTION: THD; BODY MATERIAL: STAINLESS STEEL; OPERATED: LEVER; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: TEFLON; SUPPL P/N: MBV21AA403; KKS; USED ON MBV BASE PIPING ON GT AUX SYSTEMS",null,"BALL","1/2 IN","STAINLESS STEEL","65 BAR","STAINLESS STEEL","THD",null,null,"LEVER","MBV BASE PIPING ON GT AUX SYSTEMS",null,"MBV21AA403",null,"TEFLON"]
["Ankerlig Power Station",233893,"VALVE, BALL: VALVE SIZE: 3/4 IN; DESIGN RATING: 40; CONNECTION: THD; BODY MATERIAL: STAINLESS STEEL; OPERATED: LEVER; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: TEFLON; SUPPL P/N: MBV26AA401; KKS; USED ON MBV BASE PIPING ON GT AUX SYSTEMS",null,"BALL","3/4 IN","STAINLESS STEEL",40,"STAINLESS STEEL","THD",null,null,"LEVER","MBV BASE PIPING ON GT AUX SYSTEMS",null,"MBV26AA401",null,"TEFLON"]
["Ankerlig Power Station",233895,"VALVE, RELIEF: VALVE SIZE: 3/4 X 1/2 IN; SET PRESSURE: 10 BAR; CONNECTION: BSP; BODY MATERIAL: BRASS; TRIM: BRASS; OPERATED: PRESSURE; SUPPL P/N: MBV23AA191; KKS; USED ON GT AUX SYSTEMS",null,"RELIEF","3/4 X 1/2 IN","BRASS","10 BAR","BRASS","BSP",null,null,"PRESSURE","GT AUX SYSTEMS",null,"MBV23AA191"]
["Ankerlig Power Station",233896,"VALVE: TYPE: THROTTLE; OPERATED: KEY LOCK; BODY MATERIAL: STL; REFERENCE NO: MBV31AA285; USED ON CONTROL BLOCK ON MBV BASE PIPING ON GT AUX SYSTEMS",null,"THROTTLE",null,"STL",{"$nulls":5},"KEY LOCK","CONTROL BLOCK ON MBV BASE PIPING ON GT AUX SYSTEMS",null,"MBV31AA285"]
["Ankerlig Power Station",233898,"VALVE, BALL: VALVE SIZE: 2 IN; DESIGN RATING: 40 BAR; CONNECTION: THD; BODY MATERIAL: STAINLESS STEEL; OPERATED: LEVER; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: TEFLON; SUPPL P/N: MBV10AA401; KKS; USED ON MBV BASE PIPING ON GT AUX SYSTEMS",null,"BALL","2 IN","STAINLESS STEEL","40 BAR","STAINLESS STEEL","THD",null,null,"LEVER","MBV BASE PIPING ON GT AUX SYSTEMS",null,"MBV10AA401",null,"TEFLON"]
["Ankerlig Power Station",233901,"VALVE, CHECK: TYPE: NON RETURN; VALVE SIZE: 150 MM; DESIGN RATING: 10-40 BAR; CONNECTION: FLANGE; STYLE: 1 WAY; TRIM: 1.4408; GRADE: 1.057; SUPPL P/N: MBV21AA201; KKS, USED ON MBV BASE PIPING ON GT AUX SYSTEMS",null,"CHECK; NON RETURN","150 MM",null,"10-40 BAR",1.4408,"FLANGE",{"$nulls":3},"MBV BASE PIPING ON GT AUX SYSTEMS",null,"MBV21AA201"]
["Ankerlig Power Station",235772,"VALVE: TYPE: ISOLATING GAUGE; VALVE SIZE: NB 4; DESIGN RATING: PN400; CONNECTION: THD 1/2 IN; OPERATED: MANUAL; BODY MATERIAL: 1.4571; STYLE: 1 WAY; TRIM: GR 1.4571; SOFTGOODS: GR 1.4571; WITH ONE KNOB; USED ON GAS 1 AUX SYSTEM",null,"ISOLATING GAUGE","NB 4",1.4571,"PN400","GR 1.4571","THD 1/2 IN",null,null,"MANUAL","GAS 1 AUX SYSTEM",{"$nulls":3},"GR 1.4571"]
["Ankerlig Power Station",235774,"VALVE: TYPE: ISOLATING; VALVE SIZE: 1 IN; DESIGN RATING: PN40; CONNECTION: THD 30 MM; OPERATED: MANUAL; BODY MATERIAL: STL; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: STAINLESS STEEL; SUPPL P/N: S90; USED ON GAS 1 AUX SYSTEM",null,"ISOLATING","1 IN","STL","PN40","STAINLESS STEEL","THD 30 MM",null,null,"MANUAL","GAS 1 AUX SYSTEM",null,"S90",null,"STAINLESS STEEL"]
["Ankerlig Power Station",235781,"VALVE, CHECK: VALVE SIZE: 80; DESIGN RATING: PN16; BODY MATERIAL: BRZ; OPERATED: SPRING; STYLE: 1 WAY; TRIM: DISC SS; SOFTGOODS: STAINLESS STEEL; SUPPL P/N: RK71; NON RETURN; WITH SPIRAL CENTERING RING; USED ON GAS 1 AUX SYSTEM; TEMPERATURE RATING: 13 BAR AT 250 DEG CEL",null,"CHECK",80,"BRZ","PN16","DISC SS",{"$nulls":3},"SPRING","GAS 1 AUX SYSTEM","13 BAR AT 250 DEG CEL","RK71",null,"STAINLESS STEEL"]
["Ankerlig Power Station",235783,"VALVE, RELIEF: VALVE SIZE: 3/4 IN; TEMPERATURE RATING: 130 DEG C; CONNECTION: FEMALE THD; BODY MATERIAL: CRNIMO-STAHL; OPERATED: AIR; DESIGN RATING: PN16; PRESSURE RANGE: 0-16 BAR; REFERENCE NO: 7146002; MANKENBURG; USED ON GAS 1 AUX SYSTEM.","Mankenburg","RELIEF","3/4 IN","CRNIMO-STAHL","PN16; 0-16 BAR",null,"FEMALE THD",null,null,"AIR","GAS 1 AUX SYSTEM","130 DEG C",7146002]
["Ankerlig Power Station",238889,"VALVE: TYPE: GAGE ISOLATING; VALVE SIZE: 4 MM; DESIGN RATING: PN400; CONNECTION: 1/2 IN-BSP; OPERATED: MANUAL; BODY MATERIAL: CI; STYLE: 1 WAY; TRIM: CI; REFERENCE NO: 061462-9515.002; COMPLETE WITH BLEED DOWN SCREW; USED ON GAS 1 PLANT","Wika","GAGE ISOLATING","4 MM","CI","PN400","CI","1/2 IN-BSP",null,null,"MANUAL","GAS 1 PLANT",null,"061462-9515.002"]
["Ankerlig Power Station",239052,"VALVE, BALL: VALVE SIZE: 1/2 IN; DESIGN RATING: 16 BAR; CONNECTION: THD FEMALE; BODY MATERIAL: STAINLESS STEEL; OPERATED: WING GREEN; STYLE: 1 WAY; TRIM: TEFLON; FOR USE ON GAS 1 PLANT",null,"BALL","1/2 IN","STAINLESS STEEL","16 BAR","TEFLON","THD FEMALE",null,null,"WING GREEN","GAS 1 PLANT"]
["Ankerlig Power Station",239053,"VALVE, RELIEF: VALVE SIZE: 1 IN; SET PRESSURE: 5.6 BAR; CONNECTION: THD; BODY MATERIAL: CI; OPERATED: PRESSURE; STYLE: 1 WAY; SUPPL P/N: 4593.2504; FOR USE ON GAS 1 PLANT",null,"RELIEF","1 IN","CI","5.6 BAR",null,"THD",null,null,"PRESSURE","GAS 1 PLANT",null,4593.2504]
["Ankerlig Power Station",239054,"VALVE, RELIEF: VALVE SIZE: 1 IN; SET PRESSURE: 6 BAR; CONNECTION: THD; BODY MATERIAL: CI; OPERATED: PRESSURE; STYLE: 1 WAY; SUPPL P/N: 4603.7863; TYPE SAFETY; TYPE LESER; FOR USE ON GAS 1 PLANT","SAFETY; LESER","RELIEF","1 IN","CI","6 BAR",null,"THD",null,null,"PRESSURE","GAS 1 PLANT",null,4603.7863]
["Ankerlig Power Station",239062,"VALVE, BALL: VALVE SIZE: 150 MM; CONNECTION: FLANGE; BODY MATERIAL: STL; STYLE: 1 WAY; TO BE SUPPLIED WITH ACTUATOR; FOR USE ON GAS 1 PLANT","Auma","BALL","150 MM","STL",null,null,"FLANGE",{"$nulls":3},"GAS 1 PLANT"]
["Ankerlig Power Station",239649,"VALVE, BALL: VALVE SIZE: 1/2 IN; DESIGN RATING: 16; TEMPERATURE RATING: -20 TO 130 DEG C; CONNECTION: THD 1/2 IN; BODY MATERIAL: BRS NICKEL PLTD; FACE TO FACE LENGTH: 50 MM; OPERATED: LEVER; STYLE: 1 WAY VALVE AND PLUG; APPLICATION: WATER; SUPPL P/N: 305220108",null,"BALL","1/2 IN","BRS NICKEL PLTD",16,null,"THD 1/2 IN","50 MM",null,"LEVER","WATER","-20 TO 130 DEG C",305220108]
["Ankerlig Power Station",239669,"VALVE, SOLENOID: PIPE SIZE: DN15; STYLE: 2/2 WAY; POTENTIAL: 24 VDC; DESIGN RATING: 0-40 BAR; CONNECTION: FLANGE; BODY MATERIAL: STAINLESS STEEL; OPERATED: SOLENOID; ENCLOSURE RATING: IP65; MEDIUM: DEMINIRALIZED WATER 70; POWER: 24 V X 1.6 A; CURRENT: 1.6 A; ORIFICE SIZE: DN 15; SOFTGOODS: SEAL VITON; APPLICATION: DEMIN WATER; SPECIFICATION: COAX VALVE; MANUF P/N: FK15NC; REFERENCE NO: 513465","Coax","SOLENOID","DN15; DN 15","STAINLESS STEEL","0-40 BAR",null,"FLANGE",null,null,"SOLENOID","DEMINIRALIZED WATER 70; DEMIN WATER",null,"FK15NC; 513465","24 VDC; 24 V X 1.6 A; 1.6 A; IP65","SEAL VITON"]
["Ankerlig Power Station",239684,"VALVE, RELIEF: VALVE SIZE: 1 IN; SET PRESSURE: 10 BAR; CONNECTION: THD; BODY MATERIAL: BRASS; TRIM: BRASS; OPERATED: PRESSURE; DESIGN RATING: 25 BAR; PRESSURE RANGE: 0-25 BAR; SUPPL P/N: TUVSV 03-581 18",null,"RELIEF","1 IN","BRASS","25 BAR; 0-25 BAR; 10 BAR","BRASS","THD",null,null,"PRESSURE",null,null,"TUVSV 03-581 18"]
["Ankerlig Power Station",239791,"VALVE, RELIEF: VALVE SIZE: DN 32, 140 MM; SET PRESSURE: 22 BAR; CONNECTION: FLANGE, 140 MM; BODY MATERIAL: STAINLESS STEEL; TRIM: STAINLESS STEEL; FACE TO FACE LENGTH: 275 MM; OPERATED: SPRING; APPLICATION: TURBINE PURGE WATER OVERFLOW CONTROL; GRADE: 1.4408; DESIGN RATING: PN40; VALVE MADE OF CAST STEEL; SEAT,CONE,GUID CONE SPINDLE OF HIGH QUALITY STEEL; CENTRAL SPRING, DIN PN40; WILLEM SCHLEY HAMBURG - OVERFLOW VALVE MODEL T27","WILLEM SCHLEY HAMBURG - OVERFLOW VALVE; Willem Schley","RELIEF","DN 32, 140 MM","STAINLESS STEEL","PN40; 22 BAR","STAINLESS STEEL","FLANGE, 140 MM","275 MM",null,"SPRING","TURBINE PURGE WATER OVERFLOW CONTROL",{"$nulls":3},"L"]
["Ankerlig Power Station",239795,"VALVE, CHECK: TYPE: NON RETURN; VALVE SIZE: 150 MM; DESIGN RATING: PN40; CONNECTION: FLANGE; BODY MATERIAL: STAINLESS STEEL; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SUPPL P/N: RK86A",null,"CHECK; NON RETURN","150 MM","STAINLESS STEEL","PN40","STAINLESS STEEL","FLANGE",{"$nulls":5},"RK86A"]
["Ankerlig Power Station",250048,"VALVE, CHECK: APPLICATION: CENTRIFUGES; MANUF P/N: 176289482; CAPACITY 2.8 L/MIN","Alva-Laval","CHECK",{"$nulls":8},"CENTRIFUGES",null,176289482]
["Ankerlig Power Station",250049,"VALVE, CHECK: APPLICATION: CENTRIFUGES; MANUF P/N: 176289486; OPERATED FLOW, CAPACITY 23 L/MIN","Alva-Laval","CHECK",{"$nulls":8},"CENTRIFUGES",null,176289486]
["Ankerlig Power Station",250052,"VALVE, SOLENOID: PIPE SIZE: 3/4 X 1 IN; STYLE: 4/2 WAY; POTENTIAL: 24 VDC; DESIGN RATING: 17 BAR; CONNECTION: NPT; BODY MATERIAL: BRASS; OPERATED: ELECTRONIC; ENCLOSURE RATING: IP65; MEDIUM: OIL/WATER; POWER: 11.6 W; CURRENT: 0.48 A; ORIFICE SIZE: 19 MM; COIL: SINGLE; APPLICATION: SSS CLUTCH; SPECIFICATION: SOLINOID VALVE; MANUF P/N: SC8344G076; REFERENCE NO: SC8344G076","Asco (Automatic Switch)","SOLENOID","3/4 X 1 IN; 19 MM","BRASS","17 BAR",null,"NPT",null,null,"ELECTRONIC","OIL/WATER; SSS CLUTCH",null,"SC8344G076","24 VDC; 11.6 W; 0.48 A; SINGLE; IP65"]
["Ankerlig Power Station",257026,"VALVE, BALL: VALVE SIZE: 40 MM; DESIGN RATING: 100; TEMPERATURE RATING: -10 TO 200 DEG C; CONNECTION: FLANGE; BODY MATERIAL: STEEL; FACE TO FACE LENGTH: 250; OPERATED: ACTUATOR ELECTRIC; GRADE: I54; TYPE: PREMIX","Argus","BALL; PREMIX","40 MM","STEEL",100,null,"FLANGE",250,null,"ACTUATOR ELECTRIC",null,"-10 TO 200 DEG C"]
["Ankerlig Power Station",257160,"VALVE, BALL: VALVE SIZE: 40 MM; DESIGN RATING: 100; TEMPERATURE RATING: -70 TO 300 DEG C; CONNECTION: FLANGE; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 250; OPERATED: ACTUATOR; TYPE: DIFFUSION","Argus","BALL; DIFFUSION","40 MM","STAINLESS STEEL",100,null,"FLANGE",250,null,"ACTUATOR",null,"-70 TO 300 DEG C"]
["Ankerlig Power Station",553121,"VALVE, SOLENOID: PIPE SIZE: 1/2 IN; STYLE: (2) PIPE CONNECTIONS; (1) SOLENOID; POTENTIAL: 220 VDC; DESIGN RATING: 0-100 BAR; CONNECTION: TERMINAL; BODY MATERIAL: GS/BRS; OPERATED: COIL; ENCLOSURE RATING: IP65; MEDIUM: DIESEL; POWER: 40 W; CURRENT: 0.17 A DC; ORIFICE SIZE: G 1/2 IN; COIL: 220 VOLT DC INSULATION CLASS - H; SOFTGOODS: VITON SEALS; APPLICATION: DIFFUSION/PREMIX FUEL LINES V9214 GAS TURBINES; SPECIFICATION: MK15NC2E; CLASSIFICATION: E X NA11 T3; MANUF P/N: MK15NC2E; 523181; TERMINAL 130 X M15 X 1.5 MM","Muller Coax","SOLENOID","1/2 IN; G 1/2 IN","GS/BRS","0-100 BAR",null,"TERMINAL",null,null,"COIL","DIESEL; DIFFUSION/PREMIX FUEL LINES V9214 GAS TURBINES",null,"MK15NC2E","220 VDC; 40 W; 0.17 A DC; 220 VOLT DC INSULATION CLASS - H; IP65; E X NA11 T3","VITON SEALS"]
["Ankerlig Power Station",553122,"VALVE: TYPE: SOLENOID COAXIAL; VALVE SIZE: G10/0; DESIGN RATING: 40 BAR; TEMPERATURE RATING: -40 TO 100 DEG C; CONNECTION: 1/2 IN; OPERATED: ELECTRIC COIL 220VAC; BODY MATERIAL: BRASS; SPECIFICATION: VALVE; SOFTGOODS: VITON; SPECIAL FEATURES: VITON SEAL; MANUF P/N: MK25DRN01E; 510038","Coax","SOLENOID COAXIAL","G10/0","BRASS","40 BAR",null,"1/2 IN",null,null,"ELECTRIC COIL 220VAC",null,"-40 TO 100 DEG C","MK25DRN01E",null,"VITON"]
["Ankerlig Power Station",553123,"VALVE: TYPE: SOLONOID COAXIAL; VALVE SIZE: PN40; DESIGN RATING: 0-40 BAR; TEMPERATURE RATING: -40 TO 100 DEG C; CONNECTION: FLANGE PN40; OPERATED: ELECTRIC COIL 230VAC; BODY MATERIAL: BRASS; SPECIFICATION: VALVE; SOFTGOODS: VITON; SPECIAL FEATURES: VITON SEALS; MANUF P/N: 515259; FK25NC1E","Coax","SOLONOID COAXIAL","PN40","BRASS","0-40 BAR",null,"FLANGE PN40",null,null,"ELECTRIC COIL 230VAC",null,"-40 TO 100 DEG C",515259,null,"VITON"]
["Ankerlig Power Station",553124,"VALVE: TYPE: SOLONOID COAXIAL; VALVE SIZE: PN40; DESIGN RATING: 0-40 BAR; TEMPERATURE RATING: -40 TO 100 DEG C; CONNECTION: FLANGE; OPERATED: ELECTRIC COIL 240VAC; BODY MATERIAL: BRASS; SPECIFICATION: VALVE; SOFTGOODS: VITON; SPECIAL FEATURES: VITON SEALS; MANUF P/N: 527506; FK25NC","Coax","SOLONOID COAXIAL","PN40","BRASS","0-40 BAR",null,"FLANGE",null,null,"ELECTRIC COIL 240VAC",null,"-40 TO 100 DEG C",527506,null,"VITON"]
["Ankerlig Power Station",553125,"VALVE: TYPE: SOLONOID COAXIAL; VALVE SIZE: NB8 MM; DESIGN RATING: 0-150 BAR; TEMPERATURE RATING: 55 DEG C; CONNECTION: 3/8 IN THREAD; OPERATED: ELECTRIC COIL 220VDC; BODY MATERIAL: BRASS; SPECIFICATION: VALVE; SOFTGOODS: VITON; MANUF P/N: 503507; ECD-H10NO2E","Coax","SOLONOID COAXIAL","NB8 MM","BRASS","0-150 BAR",null,"3/8 IN THREAD",null,null,"ELECTRIC COIL 220VDC",null,"55 DEG C",503507,null,"VITON"]
["Ankerlig Power Station",553126,"VALVE: TYPE: COAXIAL SOLENOID; VALVE SIZE: G11/4; 38 MM; DESIGN RATING: 0-100 BAR; TEMPERATURE RATING: -40 TO 100 DEG C; CONNECTION: 1-1/4 IN THREAD; OPERATED: ELECTRIC COIL 220VDC; BODY MATERIAL: BRASS; SOFTGOODS: VITON; MANUF P/N: 500479; MK25NC1E","Coax","COAXIAL SOLENOID","G11/4","BRASS","0-100 BAR",null,"1-1/4 IN THREAD",null,null,"ELECTRIC COIL 220VDC",null,"-40 TO 100 DEG C",500479,null,"VITON"]
["Ankerlig Power Station",553127,"VALVE: TYPE: SOLENOID COAXIAL; VALVE SIZE: PN100; DESIGN RATING: 0-100 BAR; TEMPERATURE RATING: -40 TO 100 DEG C; FACE TO FACE LENGTH: 241 MM; CONNECTION: THREAD/FLANGE; OPERATED: ELECTRIC COIL 220VDC; BODY MATERIAL: BRASS; SPECIFICATION: VALVE; SOFTGOODS: VITON; SPECIAL FEATURES: VITON SEALS; MANUF P/N: 527372; FKI5NC1E","Coax","SOLENOID COAXIAL","PN100","BRASS","0-100 BAR",null,"THREAD/FLANGE","241 MM",null,"ELECTRIC COIL 220VDC",null,"-40 TO 100 DEG C",527372,null,"VITON"]
["Ankerlig Power Station",553128,"VALVE: TYPE: SOLONOID COAXIAL; VALVE SIZE: G1/2; DESIGN RATING: 0-100 BAR; TEMPERATURE RATING: -40 TO 100 DEG C; CONNECTION: THREAD/FLANGE; OPERATED: ELECTRIC COIL 230VAC; BODY MATERIAL: BRASS; SPECIFICATION: VALVE; SOFTGOODS: VITON; MANUF P/N: MK15NC1E; 520496","Coax","SOLONOID COAXIAL","G1/2","BRASS","0-100 BAR",null,"THREAD/FLANGE",null,null,"ELECTRIC COIL 230VAC",null,"-40 TO 100 DEG C","MK15NC1E",null,"VITON"]
["Ankerlig Power Station",553129,"VALVE: TYPE: INLINE SOLENOID; VALVE SIZE: G1/2 IN-BSPP; DESIGN RATING: 0-40 BAR; TEMPERATURE RATING: -40 TO 100 DEG C; FACE TO FACE LENGTH: 184 MM; CONNECTION: THD; OPERATED: ELECTRIC COIL 220VDC; BODY MATERIAL: GS/BRS; STYLE: 2/2 WAY DIRECT ACTING; TRIM: BODY MATERIAL BRASS/GALVANISED STEEL; SPECIFICATION: VALVE; SOFTGOODS: VITON; SPECIAL FEATURES: 2 X INDUCTIVE PROXIMITY SWITCHES/SAME DIRECTION SWITCHING; MANUF P/N: 503506; MK15NC2E","Muller Coax","INLINE SOLENOID","G1/2 IN-BSPP","GS/BRS","0-40 BAR","BODY MATERIAL BRASS/GALVANISED STEEL","THD","184 MM",null,"ELECTRIC COIL 220VDC",null,"-40 TO 100 DEG C",503506,null,"VITON"]
["Ankerlig Power Station",585702,"VALVE, SOLENOID: PIPE SIZE: G3/8 IN; STYLE: 2/2 WAY; POTENTIAL: 220 VDC; DESIGN RATING: 0-150 BAR; CONNECTION: THD; BODY MATERIAL: BRASS; OPERATED: SOLENOID; ENCLOSURE RATING: IP65; MEDIUM: FUEL/OIL; ORIFICE SIZE: 10 MM; SOFTGOODS: VITON SEALS; APPLICATION: FUEL/OIL; SPECIFICATION: 516348; CLASSIFICATION: ZONE 2; MANUF P/N: ECD-H10NO2E; 2 LIMIT SWITCHES, 55 DEG; HIGH PRESSURE","Muller Coax","SOLENOID","G3/8 IN; 10 MM","BRASS","0-150 BAR",null,"THD",null,null,"SOLENOID","FUEL/OIL",null,"ECD-H10NO2E","220 VDC; IP65; ZONE 2","VITON SEALS"]
["Ankerlig Power Station",588761,"VALVE, BUTTERFLY: TYPE: SWIVEL; VALVE SIZE: 400 MM; DESIGN RATING: 6 BAR; TEMPERATURE RATING: 270 DEG C; CONNECTION: FLANGE; BODY MATERIAL: STEEL WELDMENT; FACE TO FACE LENGTH: 310 MM; OPERATED: ACTUATOR PNEUMATIC; TRIM: FLEXIBLE PRESS FORMED; SOFTGOODS: PTFE COMPOUND; APPLICATION: TURBINE COMPRESSOR; GRADE: PN10; DIN 2632; DRAWING NO: 1.5055B REV 0; INCLUDING ACTUATOR: ACTUATOR POSITION SLV 3540043 (TOP)","Friedrich Krombach","BUTTERFLY; SWIVEL","400 MM","STEEL WELDMENT","6 BAR","FLEXIBLE PRESS FORMED","FLANGE","310 MM",null,"ACTUATOR PNEUMATIC; ACTUATOR POSITION SLV 3540043 (TOP)","TURBINE COMPRESSOR","270 DEG C","1.5055B REV 0",null,"PTFE COMPOUND"]
["Ankerlig Power Station",593549,"VALVE, BUTTERFLY: TYPE: SWIVEL; VALVE SIZE: 400 MM; DESIGN RATING: 6 BAR; TEMPERATURE RATING: 270 DEG C; CONNECTION: FLANGE; BODY MATERIAL: STEEL WELDMENT; FACE TO FACE LENGTH: 310 MM; OPERATED: ACTUATOR PNEUMATIC; TRIM: FLEXIBLE PRESS FORMED; SOFTGOODS: PTFE COMPOUND; APPLICATION: TURBINE COMPRESSOR; GRADE: PN10; DIN 2632; DRAWING NO: 1.5055B REV 0; INCLUDING ACTUATOR; ACTUATOR POSITION SLV 3540041 L/H","Friedrich Krombach","BUTTERFLY; SWIVEL","400 MM","STEEL WELDMENT","6 BAR","FLEXIBLE PRESS FORMED","FLANGE","310 MM",null,"ACTUATOR PNEUMATIC","TURBINE COMPRESSOR","270 DEG C","1.5055B REV 0",null,"PTFE COMPOUND"]
["Ankerlig Power Station",593550,"VALVE, BUTTERFLY: TYPE: SWIVEL; VALVE SIZE: 400 MM; DESIGN RATING: 6 BAR; TEMPERATURE RATING: 270 DEG C; CONNECTION: FLANGE; BODY MATERIAL: STEEL WELDMENT; FACE TO FACE LENGTH: 310 MM; OPERATED: ACTUATOR PNEUMATIC; TRIM: FLEXIBLE PRESS FORMED; SOFTGOODS: PTFE COMPOUND; APPLICATION: TURBINE COMPRESSOR; GRADE: PN10; DIN 2632; DRAWING NO: 1.5055B REV 0; INCLUDING ACTUATOR; ACTUATOR POSITION SLV 3540042 R/H","Friedrich Krombach","BUTTERFLY; SWIVEL","400 MM","STEEL WELDMENT","6 BAR","FLEXIBLE PRESS FORMED","FLANGE","310 MM",null,"ACTUATOR PNEUMATIC","TURBINE COMPRESSOR","270 DEG C","1.5055B REV 0",null,"PTFE COMPOUND"]
["Ankerlig Power Station",593794,"KIT: TYPE: SEAL; APPLICATION: CHANGE OVER VALVE HDD 91; COMPRISING: O-RINGS; SUPPORT RINGS; MANUF P/N: 318517; ALL O RINGS FROM VITON MATERIAL - HDD91 CHANGE OVER VALVE",null,"SEAL",{"$nulls":8},"CHANGE OVER VALVE HDD 91",null,318517]
["Ankerlig Power Station",593797,"KIT: TYPE: SEAL; APPLICATION: CHANGE OVER VALVE HDD 170; COMPRISING: O-RINGS; SUPPORT RINGS; MANUF P/N: 308333; ALL O RINGS FROM VITON MATERIAL - HDD 170 CHANGE OVER VALVE",null,"SEAL",{"$nulls":8},"CHANGE OVER VALVE HDD 170",null,308333]
["Ankerlig Power Station",607158,"VALVE, BALL: VALVE SIZE: 40 MM; DESIGN RATING: 100 BAR; TEMPERATURE RATING: -10 TO 200 DEG C; CONNECTION: FLANGE; BODY MATERIAL: STEEL; FACE TO FACE LENGTH: 850 MM; OPERATED: ACTUATOR/ELECTRICAL; GRADE: I54; TYPE: FUEL DIFFUSION; MANUF P/N: 5100046637-100; 6211-0100-670289/G84/G82G; VALVE AND ACTUATOR ASSEMBLY","Argus","BALL; FUEL DIFFUSION","40 MM","STEEL","100 BAR",null,"FLANGE","850 MM",null,"ACTUATOR/ELECTRICAL",null,"-10 TO 200 DEG C","5100046637-100"]
["Ankerlig Power Station",612657,"VALVE, BALL: VALVE SIZE: DN 40; DESIGN RATING: PN100; TEMPERATURE RATING: -10 TO 200 DEG C; CONNECTION: FLANGE; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 300 MM; OPERATED: ELECTRICAL MOTOR; STYLE: 3 WAY; TYPE: PREMIX; SUPPL P/N: 6211-0100-670852MOD/-G85GH...M; VALVE AND ACTUATOR ASSEMBLY; ARGUS E25 ELECTRIC ACTUATOR, VALVE AND ELECTRIC ACTUATOR ASSEMBLY A2A50296201/ PB0000279980","Argus","BALL; PREMIX","DN 40","STAINLESS STEEL","PN100",null,"FLANGE","300 MM",null,"ELECTRICAL MOTOR",null,"-10 TO 200 DEG C","6211-0100-670852MOD/-G85GH...M"]
["Ankerlig Power Station",613732,"VALVE: TYPE: SOL; VALVE SIZE: 15 MM; TEMPERATURE RATING: MAX 160 DEG C; FACE TO FACE LENGTH: 130 MM; CONNECTION: FLANGE; OPERATED: ELECTRICAL; BODY MATERIAL: STAINLESS STEEL; OEM P/N: 12-EVF 5R U.XN.P.09.29; A2A50268346; SUPPL P/N: 799.010.010.0421; 220 VDC","Argus","SOL","15 MM","STAINLESS STEEL",null,null,"FLANGE","130 MM",null,"ELECTRICAL",null,"MAX 160 DEG C","12-EVF 5R U.XN.P.09.29; 799.010.010.0421"]
["Ankerlig Power Station",613733,"VALVE: TYPE: SOL; VALVE SIZE: 15 MM; TEMPERATURE RATING: MAX 160 DEG C; FACE TO FACE LENGTH: 130 MM; CONNECTION: FLANGE; OPERATED: ELECTRICAL; BODY MATERIAL: STAINLESS STEEL; OEM P/N: 12-EVDF 3R XN.W.U.P.09.29; SUPPL P/N: 799.010.010.0422; A2A50268347; 220 VDC","Uni Gerate","SOL","15 MM","STAINLESS STEEL",null,null,"FLANGE","130 MM",null,"ELECTRICAL",null,"MAX 160 DEG C","12-EVDF 3R XN.W.U.P.09.29; 799.010.010.0422"]
["Ankerlig Power Station",613741,"VALVE: TYPE: NON RETURN,WAFER; VALVE SIZE: 54 MM; DESIGN RATING: 160 BAR; TEMPERATURE RATING: 300 DEG C; FACE TO FACE LENGTH: 25 MM; CONNECTION: COUPLING; OPERATED: PNEUMATIC; BODY MATERIAL: STAINLESS STEEL; STYLE: WAFER; TRIM: DISC SS; OEM P/N: A2A50005975; SUPPL P/N: 700.050.010.1028",null,"NON RETURN,WAFER","54 MM","STAINLESS STEEL","160 BAR","DISC SS","COUPLING","25 MM",null,"PNEUMATIC",null,"300 DEG C","A2A50005975; 700.050.010.1028"]
["Ankerlig Power Station",622490,"VALVE, SOLENOID: PIPE SIZE: DN25; STYLE: 1/2; POTENTIAL: 220 V; DESIGN RATING: PN40; CONNECTION: FLANGE; BODY MATERIAL: STEEL; OPERATED: ELECTRIC; ENCLOSURE RATING: IP65; MEDIUM: BUTANE/NATURAL GAS/PROPANE; CURRENT: 0.33 A; OEM P/N: A2A50272850; SUPPL P/N: PB0000267703",null,"SOLENOID","DN25","STEEL","PN40",null,"FLANGE",null,null,"ELECTRIC","BUTANE/NATURAL GAS/PROPANE",null,"A2A50272850; PB0000267703","220 V; 0.33 A; IP65"]
["Ankerlig Power Station",622492,"VALVE, SOLENOID: PIPE SIZE: DN25; STYLE: 2/2; POTENTIAL: 230 V; DESIGN RATING: PN40; CONNECTION: FLANGE; BODY MATERIAL: STEEL; OPERATED: ELECTRIC; ENCLOSURE RATING: IP65; MEDIUM: BUTANE/NATURAL GAS/PROPANE; POWER: 160 W; CURRENT: 0.33 A; SPECIFICATION: DIN 3394-1; OEM P/N: 40-EVSADU 10NH-4 P.XN.09.20.32; SUPPL P/N: PB0000282466; A2A50296211","Uni Gerate","SOLENOID","DN25","STEEL","PN40",null,"FLANGE",null,null,"ELECTRIC","BUTANE/NATURAL GAS/PROPANE",null,"40-EVSADU 10NH-4 P.XN.09.20.32; PB0000282466","230 V; 160 W; 0.33 A; IP65"]
["Ankerlig Power Station",626656,"VALVE, CHECK: TYPE: HYDRAULIC; VALVE SIZE: G1/2 IN; DESIGN RATING: MAX 350 BAR; TEMPERATURE RATING: -30 TO 80 DEG C; CONNECTION: G1/2 IN-BSPP; BODY MATERIAL: STEEL; FACE TO FACE LENGTH: 16 MM; OPERATED: PNEUMATIC; OEM P/N: PG0031832800; SUPPL P/N: A2A50315038",null,"CHECK; HYDRAULIC","G1/2 IN","STEEL","MAX 350 BAR",null,"G1/2 IN-BSPP","16 MM",null,"PNEUMATIC",null,"-30 TO 80 DEG C","PG0031832800; A2A50315038"]
["Ankerlig Power Station",643634,"VALVE: TYPE: CONTROL; VALVE SIZE: 6 IN; DESIGN RATING: 21 BAR; TEMPERATURE RATING: 65 DEG C; FACE TO FACE LENGTH: 235 MM; CONNECTION: WAFER; OPERATED: PILOT; BODY MATERIAL: CS; SPECIFICATION: 799-D; REFERENCE NO: 139163","INBAL","CONTROL","6 IN","CS","21 BAR",null,"WAFER","235 MM",null,"PILOT",null,"65 DEG C",139163]
["Ankerlig Power Station",644167,"VALVE: TYPE: STOP; VALVE SIZE: DN 50; DESIGN RATING: 16 BAR; TEMPERATURE RATING: 120 DEG C; FACE TO FACE LENGTH: 150 MM; CONNECTION: FLANGE; OPERATED: MANUAL; BODY MATERIAL: CAST IRON; GRADE: EN-JL1040; SPECIFICATION: ARI 12072; .",null,"STOP","DN 50","CAST IRON","16 BAR",null,"FLANGE","150 MM",null,"MANUAL",null,"120 DEG C"]
["Ankerlig Power Station",644168,"VALVE: TYPE: STOP; VALVE SIZE: DN 40; DESIGN RATING: 16 BAR; TEMPERATURE RATING: 120 DEG C; FACE TO FACE LENGTH: 140 MM; CONNECTION: FLANGE 150 MM; OPERATED: MANUAL; BODY MATERIAL: CAST IRON; GRADE: EN-JL1040; SPECIFICATION: ARI 12072",null,"STOP","DN 40","CAST IRON","16 BAR",null,"FLANGE 150 MM","140 MM",null,"MANUAL",null,"120 DEG C"]
["Ankerlig Power Station",644441,"VALVE: TYPE: CONTROL; VALVE SIZE: 2 IN; DESIGN RATING: 21 BAR; TEMPERATURE RATING: 65 DEG C; FACE TO FACE LENGTH: 190 MM; CONNECTION: FLANGE; OPERATED: PILOT; BODY MATERIAL: CS; SPECIFICATION: 711-D","INBAL","CONTROL","2 IN","CS","21 BAR",null,"FLANGE","190 MM",null,"PILOT",null,"65 DEG C"]
["Ankerlig Power Station",644442,"VALVE: TYPE: CONTROL; VALVE SIZE: 3 IN; DESIGN RATING: 21 BAR; TEMPERATURE RATING: 65 DEG C; FACE TO FACE LENGTH: 155 MM; CONNECTION: WAFER; OPERATED: PILOT; BODY MATERIAL: CARBON STL; SPECIFICATION: 799-D","INBAL","CONTROL","3 IN","CARBON STL","21 BAR",null,"WAFER","155 MM",null,"PILOT",null,"65 DEG C"]
["Ankerlig Power Station",644443,"VALVE: TYPE: CONTROL; VALVE SIZE: 4 IN; DESIGN RATING: 21 BAR; TEMPERATURE RATING: 65 DEG C; FACE TO FACE LENGTH: 187 MM; CONNECTION: WAFER; OPERATED: PILOT; BODY MATERIAL: CARBON STL; SPECIFICATION: 799-D","INBAL","CONTROL","4 IN","CARBON STL","21 BAR",null,"WAFER","187 MM",null,"PILOT",null,"65 DEG C"]
["Ankerlig Power Station",647831,"VALVE, BALL: VALVE SIZE: 1 IN; DESIGN RATING: 69 BAR; TEMPERATURE RATING: 50 DEG C; CONNECTION: BSP THREADED ENDS; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 88 MM; OPERATED: MANUAL; SOFTGOODS: PTFE; PORT TYPE: FULL BORE; GRADE: ASTM A351 GR CF8M; 2 PIECE SERIES 20",null,"BALL; FULL BORE","1 IN","STAINLESS STEEL","69 BAR",null,"BSP THREADED ENDS","88 MM",null,"MANUAL",null,"50 DEG C",null,null,"PTFE"]
["Ankerlig Power Station",647833,"VALVE, BALL: VALVE SIZE: 3/4 IN; DESIGN RATING: 69; TEMPERATURE RATING: 50 DEG C; CONNECTION: BSP THREADED ENDS; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 74 MM; OPERATED: MANUAL; SOFTGOODS: PTFE; PORT TYPE: FULL BORE; GRADE: ASTM A351 GR CF8M; 2 PIECE SERIES 20",null,"BALL; FULL BORE","3/4 IN","STAINLESS STEEL",69,null,"BSP THREADED ENDS","74 MM",null,"MANUAL",null,"50 DEG C",null,null,"PTFE"]
["Ankerlig Power Station",650143,"VALVE, SOLENOID: PIPE SIZE: 3/4 IN; STYLE: 9 X CONNECTIONS; 3 X SOLENOID; POTENTIAL: 24 VDC; DESIGN RATING: 3 BAR; CONNECTION: BSP; BODY MATERIAL: BRASS; OPERATED: DIRECT SOLENOID; ENCLOSURE RATING: IP67; MEDIUM: WATER; POWER: 11.2 W; ORIFICE SIZE: 19 MM; COIL: DC; APPLICATION: CENTRIFUGE SEALING WATER; CLASSIFICATION: ZONE 2; SUPPL P/N: 176346680","Alva-Laval","SOLENOID","3/4 IN; 19 MM","BRASS","3 BAR",null,"BSP",null,null,"DIRECT SOLENOID","WATER; CENTRIFUGE SEALING WATER",null,176346680,"24 VDC; 11.2 W; DC; IP67; ZONE 2"]
["Ankerlig Power Station",671840,"VALVE, SOLENOID: PIPE SIZE: DN15; STYLE: BLOCK; POTENTIAL: 24 VDC; DESIGN RATING: 0.2-16 BAR; CONNECTION: PLUG; BODY MATERIAL: BRASS; OPERATED: DC V; ENCLOSURE RATING: IP65; MEDIUM: AIR/WATER; POWER: 11 W; CURRENT: 0.46 A; ORIFICE SIZE: 13 MM; SOFTGOODS: SEAL NBR; APPLICATION: GAS TURBINE FIRE SYSTEM; SPECIFICATION: ISO; MANUF P/N: 840131","Burkert","SOLENOID","DN15; 13 MM","BRASS","0.2-16 BAR",null,"PLUG",null,null,"DC V","AIR/WATER; GAS TURBINE FIRE SYSTEM",null,840131,"24 VDC; 11 W; 0.46 A; IP65","SEAL NBR"]
["Ankerlig Power Station",671894,"VALVE: TYPE: CHANGE OVER; VALVE SIZE: 1-1/2 IN; DESIGN RATING: 40-100 BAR; TEMPERATURE RATING: -10 TO 425 DEG C; FACE TO FACE LENGTH: 265 MM; CONNECTION: DN 40; OPERATED: HAND; BODY MATERIAL: GP 240GM + N 1.0619; STYLE: CHANGE OVER VALVE; TRIM: CR 1,4021; GRADE: CARBON STEEL; SOFTGOODS: GRAPHITE/1,4571; SPECIAL FEATURES: CHANGE OVER VALVE,3 PORTS FLANGE; PN - 300 LBS","Leser","3 PORTS FLANGE; CHANGE OVER","1-1/2 IN","GP 240GM + N 1.0619","40-100 BAR","CR 1,4021","DN 40","265 MM",null,"HAND",null,"-10 TO 425 DEG C",null,null,"GRAPHITE/1,4571"]
["Ankerlig Power Station",708469,"VALVE: TYPE: DELUGE; VALVE SIZE: 3 IN; DESIGN RATING: 21 BAR; TEMPERATURE RATING: 65 DEG C; CONNECTION: WAFER; OPERATED: ACTUATOR HYDRAULIC; BODY MATERIAL: FORGED STEEL SAE1021; INBAL MODEL 799DG-04-A01 HYDRAULIC DELGE VALVE- WAGER PATTERN ENDS RATED TO 21 TO OPEN WHEN PRESSURE IS LOST IN THE LINE, LATCH IN OPEN POSITION, LOCAL RESET COMPLETE WITH ALL NECESSARY TRIM VALVE ENDS AND WATER FLOW TEST & DRAIN ENDS DUCTILE (ASTM A53665-45-12), SLEEVE SMR5 ELATOMER REINFORCED WITH POLYESTER AND KEVLAR, CONTROL TRIM BRASS NICKEL CHROME PLATED STAINLESS STEEL AND GALVANISED STEEL","INBAL","DELUGE","3 IN","FORGED STEEL SAE1021","21 BAR",null,"WAFER",null,null,"ACTUATOR HYDRAULIC",null,"65 DEG C"]
["Ankerlig Power Station",708473,"VALVE: TYPE: DELUGE; VALVE SIZE: 4 IN; DESIGN RATING: 21 BAR; TEMPERATURE RATING: 65 DEG C; CONNECTION: WAFER; OPERATED: ACTUATOR HYDRAULIC; BODY MATERIAL: FORGED STEEL SAE1021; INBAL MODEL 799DG-04-A01 HYDRAULIC DELGE VALVE- WAGER PATTERN ENDS RATED TO 21 TO OPEN WHEN PRESSURE IS LOST IN THE LINE, LATCH IN OPEN POSITION, LOCAL RESET COMPLETE WITH ALL NECESSARY TRIM VALVE ENDS AND WATER FLOW TEST & DRAIN ENDS DUCTILE (ASTM A53665-45-12), SLEEVE SMR5 ELATOMER REINFORCED WITH POLYESTER AND KEVLAR, CONTROL TRIM BRASS NICKEL CHROME PLATED STAINLESS STEEL AND GALVANISED STEEL","INBAL","DELUGE","4 IN","FORGED STEEL SAE1021","21 BAR",null,"WAFER",null,null,"ACTUATOR HYDRAULIC",null,"65 DEG C"]
["Ankerlig Power Station",713424,"VALVE: TYPE: ISOLATING; VALVE SIZE: G1/2 IN; DESIGN RATING: 400 BAR; TEMPERATURE RATING: -20 TO 200 DEG C; FACE TO FACE LENGTH: 100 MM; CONNECTION: G1/2 IN; OPERATED: INSTRUMENT VALVE; BODY MATERIAL: STAINLESS STEEL; STYLE: VALVE WITH TEST PORT; TRIM: NEEDLE AND SEATING; GRADE: 1.4571; SPECIFICATION: DIN 16271; SOFTGOODS: CORROSION AND ACID RESISTANT; MANUF P/N: 9091157; SHUT-OFF VALVE WITH HEAT RESISTANT PLASTIC KNOB AND TEST PORT CONNECTION ,M20 X 1.5","WIKA","ISOLATING","G1/2 IN","STAINLESS STEEL","400 BAR","NEEDLE AND SEATING","G1/2 IN","100 MM",null,"INSTRUMENT VALVE",null,"-20 TO 200 DEG C",9091157,null,"CORROSION AND ACID RESISTANT; G"]
["Ankerlig Power Station",765058,"VALVE: TYPE: RELIEF; VALVE SIZE: 25 MM; DESIGN RATING: 30 BAR; TEMPERATURE RATING: 170 DEG C; CONNECTION: FLANGE MM; OPERATED: SPRING; BODY MATERIAL: CARBON",null,"RELIEF","25 MM","CARBON","30 BAR",null,"FLANGE MM",null,null,"SPRING",null,"170 DEG C"]
["Acacia Power Station",23834,"VALVE, SOLENOID: PIPE SIZE: 35 MM; STYLE: 2 WAY; POTENTIAL: 125 VDC; CONNECTION: NPT; BODY MATERIAL: STAINLESS STEEL; OPERATED: PRESSURE; ENCLOSURE RATING: IP67; MEDIUM: FUEL; SUPPL P/N: 679V100A; REFERENCE NO: 1142; 711680; FUEL SHUT OFF, MAKE ALTAIR","ALTAIR","SOLENOID","35 MM","STAINLESS STEEL",null,null,"NPT",null,null,"PRESSURE","FUEL",null,"679V100A; 1142","125 VDC; IP67"]
["Acacia Power Station",23900,"ASSEMBLY: TYPE: AIR RELEASE VALVE FILTER; DIMENSIONS: 42 IN",null,"AIR RELEASE VALVE FILTER"]
["Acacia Power Station",23909,"VALVE: TYPE: TEMPERATURE CONTROL; VALVE SIZE: 40 MM; DESIGN RATING: 150 BAR; CONNECTION: FLANGE; OPERATED: TEMPERATURE; BODY MATERIAL: STL; STYLE: BOLTED BONNET; TRIM: BONNET STL; DISC SS; GRADE: WC8; MODEL NO: 83937-3; REFERENCE NO: E76L375; RANGE: 150 - 220, MAKE ROBERSHAW","ROBERSHAW","TEMPERATURE CONTROL","40 MM","STL","150 BAR","BONNET STL","FLANGE",null,null,"TEMPERATURE",null,null,"E76L375; 83937-3"]
["Acacia Power Station",256828,"VALVE: TYPE: LIQUID FUEL METERING; VALVE SIZE: 193.5 MM2; DESIGN RATING: 345 KPA; TEMPERATURE RATING: -28 TO +103 DEG C; CONNECTION: BASE; OPERATED: ELECTRICAL; BODY MATERIAL: METAL; MANUF P/N: LQ25, 9907-361; SUPPL P/N: LQ25T","Wood Group Pratt & Whitney Industrial Turbine Services, LLC (WGPW)","LIQUID FUEL METERING","193.5 MM2","METAL","345 KPA",null,"BASE",null,null,"ELECTRICAL",null,"-28 TO +103 DEG C","LQ25, 9907-361; LQ25T"]
["Acacia Power Station",589427,"VALVE, RELIEF: VALVE SIZE: 3/4 IN; SET PRESSURE: 420 KPA; TEMPERATURE RATING: 70 DEG C; CONNECTION: THD 1/2 IN; BODY MATERIAL: BRASS; TRIM: PLASTIC BONNET/ADJUSTABLE SCREW; FACE TO FACE LENGTH: 65 MM; OPERATED: PRESSURE 0-460 KPA; DESIGN RATING: 40 BAR; PRESSURE RANGE: 0-40 BAR; MANUF P/N: D22-1/2A",null,"RELIEF","3/4 IN","BRASS","40 BAR; 0-40 BAR; 420 KPA","PLASTIC BONNET/ADJUSTABLE SCREW","THD 1/2 IN","65 MM",null,"PRESSURE 0-460 KPA",null,"70 DEG C","D22-1/2A"]

{"sheet":"Acacia Power Station","index":7,"n_rows":124,"n_cols":14,"rows_kept":124}
["Material","Original Description","OEM / Manufacturer","Valve Type","Size","Body Material","Class / Rating","Trim / Internals","End Connection","Face-to-Face","Drilling / PCD","Operation","Medium / Service","Medium Temperature"]
["0023834","VALVE, SOLENOID: PIPE SIZE: 35 MM; STYLE: 2 WAY; POTENTIAL: 125 VDC; CONNECTION: NPT; BODY MATERIAL: STAINLESS STEEL; OPERATED: PRESSURE; ENCLOSURE RATING: IP67; MEDIUM: FUEL; SUPPL P/N: 679V100A; REFERENCE NO: 1142; 711680; FUEL SHUT OFF, MAKE ALTAIR","ALTAIR","SOLENOID","35 MM","STAINLESS STEEL",null,null,"NPT",null,null,"PRESSURE","FUEL"]
["0023900","ASSEMBLY: TYPE: AIR RELEASE VALVE FILTER; DIMENSIONS: 42 IN",null,"AIR RELEASE VALVE FILTER"]
["0023909","VALVE: TYPE: TEMPERATURE CONTROL; VALVE SIZE: 40 MM; DESIGN RATING: 150 BAR; CONNECTION: FLANGE; OPERATED: TEMPERATURE; BODY MATERIAL: STL; STYLE: BOLTED BONNET; TRIM: BONNET STL; DISC SS; GRADE: WC8; MODEL NO: 83937-3; REFERENCE NO: E76L375; RANGE: 150 - 220, MAKE ROBERSHAW","ROBERSHAW","TEMPERATURE CONTROL","40 MM","STL","150 BAR","BONNET STL","FLANGE",null,null,"TEMPERATURE"]
["0256828","VALVE: TYPE: LIQUID FUEL METERING; VALVE SIZE: 193.5 MM2; DESIGN RATING: 345 KPA; TEMPERATURE RATING: -28 TO +103 DEG C; CONNECTION: BASE; OPERATED: ELECTRICAL; BODY MATERIAL: METAL; MANUF P/N: LQ25, 9907-361; SUPPL P/N: LQ25T","Wood Group Pratt & Whitney Industrial Turbine Services, LLC (WGPW)","LIQUID FUEL METERING","193.5 MM2","METAL","345 KPA",null,"BASE",null,null,"ELECTRICAL",null,"-28 TO +103 DEG C"]
["0589427","VALVE, RELIEF: VALVE SIZE: 3/4 IN; SET PRESSURE: 420 KPA; TEMPERATURE RATING: 70 DEG C; CONNECTION: THD 1/2 IN; BODY MATERIAL: BRASS; TRIM: PLASTIC BONNET/ADJUSTABLE SCREW; FACE TO FACE LENGTH: 65 MM; OPERATED: PRESSURE 0-460 KPA; DESIGN RATING: 40 BAR; PRESSURE RANGE: 0-40 BAR; MANUF P/N: D22-1/2A",null,"RELIEF","3/4 IN","BRASS","40 BAR; 0-40 BAR; 420 KPA","PLASTIC BONNET/ADJUSTABLE SCREW","THD 1/2 IN","65 MM",null,"PRESSURE 0-460 KPA",null,"70 DEG C"]
[]
["Material","Picture"]
["0589427"]
{"$rows_empty":46}
["0023900"]
{"$rows_empty":34}
["0256828"]
{"$rows_empty":32}
["0023909"]

{"sheet":"Ankerlig Power Station","index":8,"n_rows":75,"n_cols":14,"rows_kept":75}
["Material","Original Description","OEM / Manufacturer","Valve Type","Size","Body Material","Class / Rating","Trim / Internals","End Connection","Face-to-Face","Drilling / PCD","Operation","Medium / Service","Medium Temperature"]
["0074956","VALVE, BALL: VALVE SIZE: 1-1/2 IN; DESIGN RATING: 600 LB; CONNECTION: BSP; BODY MATERIAL: CS; OPERATED: MANUAL; STYLE: 2 WAY; TRIM: BALL/STEM SS GR 304; SEAT PTFE",null,"BALL","1-1/2 IN","CS","600 LB","BALL/STEM SS GR 304","BSP",null,null,"MANUAL"]
["0233792","VALVE, SOLENOID: PIPE SIZE: DN15; STYLE: 2 WAY; POTENTIAL: 220 VDC; DESIGN RATING: 100 BAR; CONNECTION: FLANGE; BODY MATERIAL: GR 1.4404/1.4571; OPERATED: NO; ENCLOSURE RATING: IP65; MEDIUM: HEIZOL; CURRENT: 0.22 A; ORIFICE SIZE: DN 15; COIL: 220 V DC; MANUF P/N: FK15NO1E; SUPPL P/N: A2A50187268; REFERENCE NO: PB0000144283; 503443; 2.5 M3/HR; WITH 4 X 14 MM DIA HOLES DRILLED INTO FLANGE","Muller Coax","SOLENOID","DN15; DN 15","GR 1.4404/1.4571","100 BAR",null,"FLANGE",null,null,"NO","HEIZOL"]
["0233844","VALVE, CHECK: BODY MATERIAL: CI; SUPPL P/N: MBV30AA201; C5V08311B5; LIFTING OIL; KKS; FOR USE ON LIFTING OIL PUMP MBV BASE PIPING ON GT AUX SYSTEM","Parker","CHECK",null,"CI",{"$nulls":6},"LIFTING OIL PUMP MBV BASE PIPING ON GT AUX SYSTEM"]
["0233849","VALVE, BALL: VALVE SIZE: 1 IN; DESIGN RATING: 40 BAR; CONNECTION: BSP; BODY MATERIAL: STAINLESS STEEL; OPERATED: LEVER; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: PTFE; SUPPL P/N: MBV23AA412; REFERENCE NO: SLV3800141; MBV25AA401; WITH ATTACHMENT, KKS; FOR USE ON LUBE OIL FILTER ON MBV BASE PIPING ON GT AUX SYSTEM",null,"BALL","1 IN","STAINLESS STEEL","40 BAR","STAINLESS STEEL","BSP",null,null,"LEVER","LUBE OIL FILTER ON MBV BASE PIPING ON GT AUX SYSTEM"]
["0233850","VALVE: TYPE: ISOLATING; VALVE SIZE: NB 4; DESIGN RATING: 400 BAR; CONNECTION: BSP; OPERATED: HANDWHEEL; BODY MATERIAL: 1.046; STYLE: ISOLATE/VENT; REFERENCE NO: MBV31AA301; MBV31AA305; MBV21AA301; MBV23AA301; FOR USE ON GT AUX SYSTEMS",null,"ISOLATING","NB 4","1.046","400 BAR",null,"BSP",null,null,"HANDWHEEL","GT AUX SYSTEMS"]
["0233851","VALVE: TYPE: BALANCE; VALVE SIZE: 3/8 IN; DESIGN RATING: 16 BAR; TEMPERATURE RATING: 80-100 DEG C; CONNECTION: 3/8 IN-BSPP; OPERATED: KNOB; BODY MATERIAL: STL HARDENED BS 970; SPECIFICATION: 305000; SPECIAL FEATURES: HAND WHEEL; STL VERSION; MANUF P/N: 305000; REFERENCE NO: SLV3800141; MBV25AA252; FOR USE ON LUBE OIL FILTER ON MBV BASE PIPING ON GT AUX SYSTEM",null,"BALANCE","3/8 IN","STL HARDENED BS 970","16 BAR",null,"3/8 IN-BSPP",null,null,"KNOB","LUBE OIL FILTER ON MBV BASE PIPING ON GT AUX SYSTEM","80-100 DEG C"]
["0233857","VALVE, BUTTERFLY: TYPE: WAFER; VALVE SIZE: 150 MM; DESIGN RATING: PN16; TEMPERATURE RATING: -10 TO 80 DEG C; CONNECTION: FLANGE; BODY MATERIAL: STEEL; OPERATED: HANDLEVER; TRIM: STAINLESS STEEL; SOFTGOODS: RUBBER; REFERENCE NO: MBV21AA254; ECLS 71391; FOR USE ON MBV BASE PIPING ON GT AUX SYSTEM",null,"BUTTERFLY; WAFER","150 MM","STEEL","PN16","STAINLESS STEEL","FLANGE",null,null,"HANDLEVER","MBV BASE PIPING ON GT AUX SYSTEM","-10 TO 80 DEG C"]
["0233859","VALVE: TYPE: THROTTLE; CONNECTION: BOLTED; OPERATED: SCREW DOWN; BODY MATERIAL: STL; STYLE: 1 WAY; TRIM: STL; REFERENCE NO: MBV22AA281; FOR MBV BASE PIPING ON GT AUX SYSTEM",null,"THROTTLE",null,"STL",null,"STL","BOLTED",null,null,"SCREW DOWN"]
["0233871","VALVE, RELIEF: BODY MATERIAL: CAST IRON; DESIGN RATING: 210 BAR; SUPPL P/N: MBA30AA191; R5V 08 593 32 A5 152 210; REFERENCE NO: SLV 3720522; PARKER; KKS: FOR LIFTING OIL PUMP ON GT AUX SYSTEM","Parker","RELIEF",null,"CAST IRON","210 BAR"]
["0233872","VALVE, RELIEF: BODY MATERIAL: CI; SUPPL P/N: R4V06 535 30 A5; MBV31AA151; REFERENCE NO: SLV3860114; PARKER, KKS; FOR CONTROL BLOCK LIFTING OIL ON MBV BASE PIPING ON GT AUX SYSTEM","Parker","RELIEF",null,"CI"]
["0233891","VALVE, BALL: VALVE SIZE: 1/4 IN; DESIGN RATING: 65; CONNECTION: THD; BODY MATERIAL: STAINLESS STEEL; OPERATED: LEVER; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: TEFLON; SUPPL P/N: MBV50AA503; KKS; USED ON MBV BASE PIPING ON GT AUX SYSTEMS",null,"BALL","1/4 IN","STAINLESS STEEL","65","STAINLESS STEEL","THD",null,null,"LEVER","MBV BASE PIPING ON GT AUX SYSTEMS"]
["0233892","VALVE, BALL: VALVE SIZE: 1/2 IN; DESIGN RATING: 65 BAR; CONNECTION: THD; BODY MATERIAL: STAINLESS STEEL; OPERATED: LEVER; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: TEFLON; SUPPL P/N: MBV21AA403; KKS; USED ON MBV BASE PIPING ON GT AUX SYSTEMS",null,"BALL","1/2 IN","STAINLESS STEEL","65 BAR","STAINLESS STEEL","THD",null,null,"LEVER","MBV BASE PIPING ON GT AUX SYSTEMS"]
["0233893","VALVE, BALL: VALVE SIZE: 3/4 IN; DESIGN RATING: 40; CONNECTION: THD; BODY MATERIAL: STAINLESS STEEL; OPERATED: LEVER; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: TEFLON; SUPPL P/N: MBV26AA401; KKS; USED ON MBV BASE PIPING ON GT AUX SYSTEMS",null,"BALL","3/4 IN","STAINLESS STEEL","40","STAINLESS STEEL","THD",null,null,"LEVER","MBV BASE PIPING ON GT AUX SYSTEMS"]
["0233895","VALVE, RELIEF: VALVE SIZE: 3/4 X 1/2 IN; SET PRESSURE: 10 BAR; CONNECTION: BSP; BODY MATERIAL: BRASS; TRIM: BRASS; OPERATED: PRESSURE; SUPPL P/N: MBV23AA191; KKS; USED ON GT AUX SYSTEMS",null,"RELIEF","3/4 X 1/2 IN","BRASS","10 BAR","BRASS","BSP",null,null,"PRESSURE","GT AUX SYSTEMS"]
["0233896","VALVE: TYPE: THROTTLE; OPERATED: KEY LOCK; BODY MATERIAL: STL; REFERENCE NO: MBV31AA285; USED ON CONTROL BLOCK ON MBV BASE PIPING ON GT AUX SYSTEMS",null,"THROTTLE",null,"STL",{"$nulls":5},"KEY LOCK","CONTROL BLOCK ON MBV BASE PIPING ON GT AUX SYSTEMS"]
["0233898","VALVE, BALL: VALVE SIZE: 2 IN; DESIGN RATING: 40 BAR; CONNECTION: THD; BODY MATERIAL: STAINLESS STEEL; OPERATED: LEVER; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: TEFLON; SUPPL P/N: MBV10AA401; KKS; USED ON MBV BASE PIPING ON GT AUX SYSTEMS",null,"BALL","2 IN","STAINLESS STEEL","40 BAR","STAINLESS STEEL","THD",null,null,"LEVER","MBV BASE PIPING ON GT AUX SYSTEMS"]
["0233901","VALVE, CHECK: TYPE: NON RETURN; VALVE SIZE: 150 MM; DESIGN RATING: 10-40 BAR; CONNECTION: FLANGE; STYLE: 1 WAY; TRIM: 1.4408; GRADE: 1.057; SUPPL P/N: MBV21AA201; KKS, USED ON MBV BASE PIPING ON GT AUX SYSTEMS",null,"CHECK; NON RETURN","150 MM",null,"10-40 BAR","1.4408","FLANGE",{"$nulls":3},"MBV BASE PIPING ON GT AUX SYSTEMS"]
["0235772","VALVE: TYPE: ISOLATING GAUGE; VALVE SIZE: NB 4; DESIGN RATING: PN400; CONNECTION: THD 1/2 IN; OPERATED: MANUAL; BODY MATERIAL: 1.4571; STYLE: 1 WAY; TRIM: GR 1.4571; SOFTGOODS: GR 1.4571; WITH ONE KNOB; USED ON GAS 1 AUX SYSTEM",null,"ISOLATING GAUGE","NB 4","1.4571","PN400","GR 1.4571","THD 1/2 IN",null,null,"MANUAL","GAS 1 AUX SYSTEM"]
["0235774","VALVE: TYPE: ISOLATING; VALVE SIZE: 1 IN; DESIGN RATING: PN40; CONNECTION: THD 30 MM; OPERATED: MANUAL; BODY MATERIAL: STL; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: STAINLESS STEEL; SUPPL P/N: S90; USED ON GAS 1 AUX SYSTEM",null,"ISOLATING","1 IN","STL","PN40","STAINLESS STEEL","THD 30 MM",null,null,"MANUAL","GAS 1 AUX SYSTEM"]
["0235781","VALVE, CHECK: VALVE SIZE: 80; DESIGN RATING: PN16; BODY MATERIAL: BRZ; OPERATED: SPRING; STYLE: 1 WAY; TRIM: DISC SS; SOFTGOODS: STAINLESS STEEL; SUPPL P/N: RK71; NON RETURN; WITH SPIRAL CENTERING RING; USED ON GAS 1 AUX SYSTEM; TEMPERATURE RATING: 13 BAR AT 250 DEG CEL",null,"CHECK","80","BRZ","PN16","DISC SS",{"$nulls":3},"SPRING","GAS 1 AUX SYSTEM","13 BAR AT 250 DEG CEL"]
["0235783","VALVE, RELIEF: VALVE SIZE: 3/4 IN; TEMPERATURE RATING: 130 DEG C; CONNECTION: FEMALE THD; BODY MATERIAL: CRNIMO-STAHL; OPERATED: AIR; DESIGN RATING: PN16; PRESSURE RANGE: 0-16 BAR; REFERENCE NO: 7146002; MANKENBURG; USED ON GAS 1 AUX SYSTEM.","Mankenburg","RELIEF","3/4 IN","CRNIMO-STAHL","PN16; 0-16 BAR",null,"FEMALE THD",null,null,"AIR","GAS 1 AUX SYSTEM","130 DEG C"]
["0238889","VALVE: TYPE: GAGE ISOLATING; VALVE SIZE: 4 MM; DESIGN RATING: PN400; CONNECTION: 1/2 IN-BSP; OPERATED: MANUAL; BODY MATERIAL: CI; STYLE: 1 WAY; TRIM: CI; REFERENCE NO: 061462-9515.002; COMPLETE WITH BLEED DOWN SCREW; USED ON GAS 1 PLANT","Wika","GAGE ISOLATING","4 MM","CI","PN400","CI","1/2 IN-BSP",null,null,"MANUAL","GAS 1 PLANT"]
["0239052","VALVE, BALL: VALVE SIZE: 1/2 IN; DESIGN RATING: 16 BAR; CONNECTION: THD FEMALE; BODY MATERIAL: STAINLESS STEEL; OPERATED: WING GREEN; STYLE: 1 WAY; TRIM: TEFLON; FOR USE ON GAS 1 PLANT",null,"BALL","1/2 IN","STAINLESS STEEL","16 BAR","TEFLON","THD FEMALE",null,null,"WING GREEN","GAS 1 PLANT"]
["0239053","VALVE, RELIEF: VALVE SIZE: 1 IN; SET PRESSURE: 5.6 BAR; CONNECTION: THD; BODY MATERIAL: CI; OPERATED: PRESSURE; STYLE: 1 WAY; SUPPL P/N: 4593.2504; FOR USE ON GAS 1 PLANT",null,"RELIEF","1 IN","CI","5.6 BAR",null,"THD",null,null,"PRESSURE","GAS 1 PLANT"]
["0239054","VALVE, RELIEF: VALVE SIZE: 1 IN; SET PRESSURE: 6 BAR; CONNECTION: THD; BODY MATERIAL: CI; OPERATED: PRESSURE; STYLE: 1 WAY; SUPPL P/N: 4603.7863; TYPE SAFETY; TYPE LESER; FOR USE ON GAS 1 PLANT","SAFETY; LESER","RELIEF","1 IN","CI","6 BAR",null,"THD",null,null,"PRESSURE","GAS 1 PLANT"]
["0239062","VALVE, BALL: VALVE SIZE: 150 MM; CONNECTION: FLANGE; BODY MATERIAL: STL; STYLE: 1 WAY; TO BE SUPPLIED WITH ACTUATOR; FOR USE ON GAS 1 PLANT","Auma","BALL","150 MM","STL",null,null,"FLANGE",{"$nulls":3},"GAS 1 PLANT"]
["0239649","VALVE, BALL: VALVE SIZE: 1/2 IN; DESIGN RATING: 16; TEMPERATURE RATING: -20 TO 130 DEG C; CONNECTION: THD 1/2 IN; BODY MATERIAL: BRS NICKEL PLTD; FACE TO FACE LENGTH: 50 MM; OPERATED: LEVER; STYLE: 1 WAY VALVE AND PLUG; APPLICATION: WATER; SUPPL P/N: 305220108",null,"BALL","1/2 IN","BRS NICKEL PLTD","16",null,"THD 1/2 IN","50 MM",null,"LEVER","WATER","-20 TO 130 DEG C"]
["0239669","VALVE, SOLENOID: PIPE SIZE: DN15; STYLE: 2/2 WAY; POTENTIAL: 24 VDC; DESIGN RATING: 0-40 BAR; CONNECTION: FLANGE; BODY MATERIAL: STAINLESS STEEL; OPERATED: SOLENOID; ENCLOSURE RATING: IP65; MEDIUM: DEMINIRALIZED WATER 70; POWER: 24 V X 1.6 A; CURRENT: 1.6 A; ORIFICE SIZE: DN 15; SOFTGOODS: SEAL VITON; APPLICATION: DEMIN WATER; SPECIFICATION: COAX VALVE; MANUF P/N: FK15NC; REFERENCE NO: 513465","Coax","SOLENOID","DN15; DN 15","STAINLESS STEEL","0-40 BAR",null,"FLANGE",null,null,"SOLENOID","DEMINIRALIZED WATER 70; DEMIN WATER"]
["0239684","VALVE, RELIEF: VALVE SIZE: 1 IN; SET PRESSURE: 10 BAR; CONNECTION: THD; BODY MATERIAL: BRASS; TRIM: BRASS; OPERATED: PRESSURE; DESIGN RATING: 25 BAR; PRESSURE RANGE: 0-25 BAR; SUPPL P/N: TUVSV 03-581 18",null,"RELIEF","1 IN","BRASS","25 BAR; 0-25 BAR; 10 BAR","BRASS","THD",null,null,"PRESSURE"]
["0239791","VALVE, RELIEF: VALVE SIZE: DN 32, 140 MM; SET PRESSURE: 22 BAR; CONNECTION: FLANGE, 140 MM; BODY MATERIAL: STAINLESS STEEL; TRIM: STAINLESS STEEL; FACE TO FACE LENGTH: 275 MM; OPERATED: SPRING; APPLICATION: TURBINE PURGE WATER OVERFLOW CONTROL; GRADE: 1.4408; DESIGN RATING: PN40; VALVE MADE OF CAST STEEL; SEAT,CONE,GUID CONE SPINDLE OF HIGH QUALITY STEEL; CENTRAL SPRING, DIN PN40; WILLEM SCHLEY HAMBURG - OVERFLOW VALVE MODEL T27","WILLEM SCHLEY HAMBURG - OVERFLOW VALVE; Willem Schley","RELIEF","DN 32, 140 MM","STAINLESS STEEL","PN40; 22 BAR","STAINLESS STEEL","FLANGE, 140 MM","275 MM",null,"SPRING","TURBINE PURGE WATER OVERFLOW CONTROL"]
["0239795","VALVE, CHECK: TYPE: NON RETURN; VALVE SIZE: 150 MM; DESIGN RATING: PN40; CONNECTION: FLANGE; BODY MATERIAL: STAINLESS STEEL; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SUPPL P/N: RK86A",null,"CHECK; NON RETURN","150 MM","STAINLESS STEEL","PN40","STAINLESS STEEL","FLANGE"]
["0250048","VALVE, CHECK: APPLICATION: CENTRIFUGES; MANUF P/N: 176289482; CAPACITY 2.8 L/MIN","Alva-Laval","CHECK",{"$nulls":8},"CENTRIFUGES"]
["0250049","VALVE, CHECK: APPLICATION: CENTRIFUGES; MANUF P/N: 176289486; OPERATED FLOW, CAPACITY 23 L/MIN","Alva-Laval","CHECK",{"$nulls":8},"CENTRIFUGES"]
["0250052","VALVE, SOLENOID: PIPE SIZE: 3/4 X 1 IN; STYLE: 4/2 WAY; POTENTIAL: 24 VDC; DESIGN RATING: 17 BAR; CONNECTION: NPT; BODY MATERIAL: BRASS; OPERATED: ELECTRONIC; ENCLOSURE RATING: IP65; MEDIUM: OIL/WATER; POWER: 11.6 W; CURRENT: 0.48 A; ORIFICE SIZE: 19 MM; COIL: SINGLE; APPLICATION: SSS CLUTCH; SPECIFICATION: SOLINOID VALVE; MANUF P/N: SC8344G076; REFERENCE NO: SC8344G076","Asco (Automatic Switch)","SOLENOID","3/4 X 1 IN; 19 MM","BRASS","17 BAR",null,"NPT",null,null,"ELECTRONIC","OIL/WATER; SSS CLUTCH"]
["0257026","VALVE, BALL: VALVE SIZE: 40 MM; DESIGN RATING: 100; TEMPERATURE RATING: -10 TO 200 DEG C; CONNECTION: FLANGE; BODY MATERIAL: STEEL; FACE TO FACE LENGTH: 250; OPERATED: ACTUATOR ELECTRIC; GRADE: I54; TYPE: PREMIX","Argus","BALL; PREMIX","40 MM","STEEL","100",null,"FLANGE","250",null,"ACTUATOR ELECTRIC",null,"-10 TO 200 DEG C"]
["0257160","VALVE, BALL: VALVE SIZE: 40 MM; DESIGN RATING: 100; TEMPERATURE RATING: -70 TO 300 DEG C; CONNECTION: FLANGE; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 250; OPERATED: ACTUATOR; TYPE: DIFFUSION","Argus","BALL; DIFFUSION","40 MM","STAINLESS STEEL","100",null,"FLANGE","250",null,"ACTUATOR",null,"-70 TO 300 DEG C"]
["0553121","VALVE, SOLENOID: PIPE SIZE: 1/2 IN; STYLE: (2) PIPE CONNECTIONS; (1) SOLENOID; POTENTIAL: 220 VDC; DESIGN RATING: 0-100 BAR; CONNECTION: TERMINAL; BODY MATERIAL: GS/BRS; OPERATED: COIL; ENCLOSURE RATING: IP65; MEDIUM: DIESEL; POWER: 40 W; CURRENT: 0.17 A DC; ORIFICE SIZE: G 1/2 IN; COIL: 220 VOLT DC INSULATION CLASS - H; SOFTGOODS: VITON SEALS; APPLICATION: DIFFUSION/PREMIX FUEL LINES V9214 GAS TURBINES; SPECIFICATION: MK15NC2E; CLASSIFICATION: E X NA11 T3; MANUF P/N: MK15NC2E; 523181; TERMINAL 130 X M15 X 1.5 MM","Muller Coax","SOLENOID","1/2 IN; G 1/2 IN","GS/BRS","0-100 BAR",null,"TERMINAL",null,null,"COIL","DIESEL; DIFFUSION/PREMIX FUEL LINES V9214 GAS TURBINES"]
["0553122","VALVE: TYPE: SOLENOID COAXIAL; VALVE SIZE: G10/0; DESIGN RATING: 40 BAR; TEMPERATURE RATING: -40 TO 100 DEG C; CONNECTION: 1/2 IN; OPERATED: ELECTRIC COIL 220VAC; BODY MATERIAL: BRASS; SPECIFICATION: VALVE; SOFTGOODS: VITON; SPECIAL FEATURES: VITON SEAL; MANUF P/N: MK25DRN01E; 510038","Coax","SOLENOID COAXIAL","G10/0","BRASS","40 BAR",null,"1/2 IN",null,null,"ELECTRIC COIL 220VAC",null,"-40 TO 100 DEG C"]
["0553123","VALVE: TYPE: SOLONOID COAXIAL; VALVE SIZE: PN40; DESIGN RATING: 0-40 BAR; TEMPERATURE RATING: -40 TO 100 DEG C; CONNECTION: FLANGE PN40; OPERATED: ELECTRIC COIL 230VAC; BODY MATERIAL: BRASS; SPECIFICATION: VALVE; SOFTGOODS: VITON; SPECIAL FEATURES: VITON SEALS; MANUF P/N: 515259; FK25NC1E","Coax","SOLONOID COAXIAL","PN40","BRASS","0-40 BAR",null,"FLANGE PN40",null,null,"ELECTRIC COIL 230VAC",null,"-40 TO 100 DEG C"]
["0553124","VALVE: TYPE: SOLONOID COAXIAL; VALVE SIZE: PN40; DESIGN RATING: 0-40 BAR; TEMPERATURE RATING: -40 TO 100 DEG C; CONNECTION: FLANGE; OPERATED: ELECTRIC COIL 240VAC; BODY MATERIAL: BRASS; SPECIFICATION: VALVE; SOFTGOODS: VITON; SPECIAL FEATURES: VITON SEALS; MANUF P/N: 527506; FK25NC","Coax","SOLONOID COAXIAL","PN40","BRASS","0-40 BAR",null,"FLANGE",null,null,"ELECTRIC COIL 240VAC",null,"-40 TO 100 DEG C"]
["0553125","VALVE: TYPE: SOLONOID COAXIAL; VALVE SIZE: NB8 MM; DESIGN RATING: 0-150 BAR; TEMPERATURE RATING: 55 DEG C; CONNECTION: 3/8 IN THREAD; OPERATED: ELECTRIC COIL 220VDC; BODY MATERIAL: BRASS; SPECIFICATION: VALVE; SOFTGOODS: VITON; MANUF P/N: 503507; ECD-H10NO2E","Coax","SOLONOID COAXIAL","NB8 MM","BRASS","0-150 BAR",null,"3/8 IN THREAD",null,null,"ELECTRIC COIL 220VDC",null,"55 DEG C"]
["0553126","VALVE: TYPE: COAXIAL SOLENOID; VALVE SIZE: G11/4; 38 MM; DESIGN RATING: 0-100 BAR; TEMPERATURE RATING: -40 TO 100 DEG C; CONNECTION: 1-1/4 IN THREAD; OPERATED: ELECTRIC COIL 220VDC; BODY MATERIAL: BRASS; SOFTGOODS: VITON; MANUF P/N: 500479; MK25NC1E","Coax","COAXIAL SOLENOID","G11/4","BRASS","0-100 BAR",null,"1-1/4 IN THREAD",null,null,"ELECTRIC COIL 220VDC",null,"-40 TO 100 DEG C"]
["0553127","VALVE: TYPE: SOLENOID COAXIAL; VALVE SIZE: PN100; DESIGN RATING: 0-100 BAR; TEMPERATURE RATING: -40 TO 100 DEG C; FACE TO FACE LENGTH: 241 MM; CONNECTION: THREAD/FLANGE; OPERATED: ELECTRIC COIL 220VDC; BODY MATERIAL: BRASS; SPECIFICATION: VALVE; SOFTGOODS: VITON; SPECIAL FEATURES: VITON SEALS; MANUF P/N: 527372; FKI5NC1E","Coax","SOLENOID COAXIAL","PN100","BRASS","0-100 BAR",null,"THREAD/FLANGE","241 MM",null,"ELECTRIC COIL 220VDC",null,"-40 TO 100 DEG C"]
["0553128","VALVE: TYPE: SOLONOID COAXIAL; VALVE SIZE: G1/2; DESIGN RATING: 0-100 BAR; TEMPERATURE RATING: -40 TO 100 DEG C; CONNECTION: THREAD/FLANGE; OPERATED: ELECTRIC COIL 230VAC; BODY MATERIAL: BRASS; SPECIFICATION: VALVE; SOFTGOODS: VITON; MANUF P/N: MK15NC1E; 520496","Coax","SOLONOID COAXIAL","G1/2","BRASS","0-100 BAR",null,"THREAD/FLANGE",null,null,"ELECTRIC COIL 230VAC",null,"-40 TO 100 DEG C"]
["0553129","VALVE: TYPE: INLINE SOLENOID; VALVE SIZE: G1/2 IN-BSPP; DESIGN RATING: 0-40 BAR; TEMPERATURE RATING: -40 TO 100 DEG C; FACE TO FACE LENGTH: 184 MM; CONNECTION: THD; OPERATED: ELECTRIC COIL 220VDC; BODY MATERIAL: GS/BRS; STYLE: 2/2 WAY DIRECT ACTING; TRIM: BODY MATERIAL BRASS/GALVANISED STEEL; SPECIFICATION: VALVE; SOFTGOODS: VITON; SPECIAL FEATURES: 2 X INDUCTIVE PROXIMITY SWITCHES/SAME DIRECTION SWITCHING; MANUF P/N: 503506; MK15NC2E","Muller Coax","INLINE SOLENOID","G1/2 IN-BSPP","GS/BRS","0-40 BAR","BODY MATERIAL BRASS/GALVANISED STEEL","THD","184 MM",null,"ELECTRIC COIL 220VDC",null,"-40 TO 100 DEG C"]
["0585702","VALVE, SOLENOID: PIPE SIZE: G3/8 IN; STYLE: 2/2 WAY; POTENTIAL: 220 VDC; DESIGN RATING: 0-150 BAR; CONNECTION: THD; BODY MATERIAL: BRASS; OPERATED: SOLENOID; ENCLOSURE RATING: IP65; MEDIUM: FUEL/OIL; ORIFICE SIZE: 10 MM; SOFTGOODS: VITON SEALS; APPLICATION: FUEL/OIL; SPECIFICATION: 516348; CLASSIFICATION: ZONE 2; MANUF P/N: ECD-H10NO2E; 2 LIMIT SWITCHES, 55 DEG; HIGH PRESSURE","Muller Coax","SOLENOID","G3/8 IN; 10 MM","BRASS","0-150 BAR",null,"THD",null,null,"SOLENOID","FUEL/OIL"]
["0588761","VALVE, BUTTERFLY: TYPE: SWIVEL; VALVE SIZE: 400 MM; DESIGN RATING: 6 BAR; TEMPERATURE RATING: 270 DEG C; CONNECTION: FLANGE; BODY MATERIAL: STEEL WELDMENT; FACE TO FACE LENGTH: 310 MM; OPERATED: ACTUATOR PNEUMATIC; TRIM: FLEXIBLE PRESS FORMED; SOFTGOODS: PTFE COMPOUND; APPLICATION: TURBINE COMPRESSOR; GRADE: PN10; DIN 2632; DRAWING NO: 1.5055B REV 0; INCLUDING ACTUATOR: ACTUATOR POSITION SLV 3540043 (TOP)","Friedrich Krombach","BUTTERFLY; SWIVEL","400 MM","STEEL WELDMENT","6 BAR","FLEXIBLE PRESS FORMED","FLANGE","310 MM",null,"ACTUATOR PNEUMATIC; ACTUATOR POSITION SLV 3540043 (TOP)","TURBINE COMPRESSOR","270 DEG C"]
["0593549","VALVE, BUTTERFLY: TYPE: SWIVEL; VALVE SIZE: 400 MM; DESIGN RATING: 6 BAR; TEMPERATURE RATING: 270 DEG C; CONNECTION: FLANGE; BODY MATERIAL: STEEL WELDMENT; FACE TO FACE LENGTH: 310 MM; OPERATED: ACTUATOR PNEUMATIC; TRIM: FLEXIBLE PRESS FORMED; SOFTGOODS: PTFE COMPOUND; APPLICATION: TURBINE COMPRESSOR; GRADE: PN10; DIN 2632; DRAWING NO: 1.5055B REV 0; INCLUDING ACTUATOR; ACTUATOR POSITION SLV 3540041 L/H","Friedrich Krombach","BUTTERFLY; SWIVEL","400 MM","STEEL WELDMENT","6 BAR","FLEXIBLE PRESS FORMED","FLANGE","310 MM",null,"ACTUATOR PNEUMATIC","TURBINE COMPRESSOR","270 DEG C"]
["0593550","VALVE, BUTTERFLY: TYPE: SWIVEL; VALVE SIZE: 400 MM; DESIGN RATING: 6 BAR; TEMPERATURE RATING: 270 DEG C; CONNECTION: FLANGE; BODY MATERIAL: STEEL WELDMENT; FACE TO FACE LENGTH: 310 MM; OPERATED: ACTUATOR PNEUMATIC; TRIM: FLEXIBLE PRESS FORMED; SOFTGOODS: PTFE COMPOUND; APPLICATION: TURBINE COMPRESSOR; GRADE: PN10; DIN 2632; DRAWING NO: 1.5055B REV 0; INCLUDING ACTUATOR; ACTUATOR POSITION SLV 3540042 R/H","Friedrich Krombach","BUTTERFLY; SWIVEL","400 MM","STEEL WELDMENT","6 BAR","FLEXIBLE PRESS FORMED","FLANGE","310 MM",null,"ACTUATOR PNEUMATIC","TURBINE COMPRESSOR","270 DEG C"]
["0593794","KIT: TYPE: SEAL; APPLICATION: CHANGE OVER VALVE HDD 91; COMPRISING: O-RINGS; SUPPORT RINGS; MANUF P/N: 318517; ALL O RINGS FROM VITON MATERIAL - HDD91 CHANGE OVER VALVE",null,"SEAL",{"$nulls":8},"CHANGE OVER VALVE HDD 91"]
["0593797","KIT: TYPE: SEAL; APPLICATION: CHANGE OVER VALVE HDD 170; COMPRISING: O-RINGS; SUPPORT RINGS; MANUF P/N: 308333; ALL O RINGS FROM VITON MATERIAL - HDD 170 CHANGE OVER VALVE",null,"SEAL",{"$nulls":8},"CHANGE OVER VALVE HDD 170"]
["0607158","VALVE, BALL: VALVE SIZE: 40 MM; DESIGN RATING: 100 BAR; TEMPERATURE RATING: -10 TO 200 DEG C; CONNECTION: FLANGE; BODY MATERIAL: STEEL; FACE TO FACE LENGTH: 850 MM; OPERATED: ACTUATOR/ELECTRICAL; GRADE: I54; TYPE: FUEL DIFFUSION; MANUF P/N: 5100046637-100; 6211-0100-670289/G84/G82G; VALVE AND ACTUATOR ASSEMBLY","Argus","BALL; FUEL DIFFUSION","40 MM","STEEL","100 BAR",null,"FLANGE","850 MM",null,"ACTUATOR/ELECTRICAL",null,"-10 TO 200 DEG C"]
["0612657","VALVE, BALL: VALVE SIZE: DN 40; DESIGN RATING: PN100; TEMPERATURE RATING: -10 TO 200 DEG C; CONNECTION: FLANGE; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 300 MM; OPERATED: ELECTRICAL MOTOR; STYLE: 3 WAY; TYPE: PREMIX; SUPPL P/N: 6211-0100-670852MOD/-G85GH...M; VALVE AND ACTUATOR ASSEMBLY; ARGUS E25 ELECTRIC ACTUATOR, VALVE AND ELECTRIC ACTUATOR ASSEMBLY A2A50296201/ PB0000279980","Argus","BALL; PREMIX","DN 40","STAINLESS STEEL","PN100",null,"FLANGE","300 MM",null,"ELECTRICAL MOTOR",null,"-10 TO 200 DEG C"]
["0613732","VALVE: TYPE: SOL; VALVE SIZE: 15 MM; TEMPERATURE RATING: MAX 160 DEG C; FACE TO FACE LENGTH: 130 MM; CONNECTION: FLANGE; OPERATED: ELECTRICAL; BODY MATERIAL: STAINLESS STEEL; OEM P/N: 12-EVF 5R U.XN.P.09.29; A2A50268346; SUPPL P/N: 799.010.010.0421; 220 VDC","Argus","SOL","15 MM","STAINLESS STEEL",null,null,"FLANGE","130 MM",null,"ELECTRICAL",null,"MAX 160 DEG C"]
["0613733","VALVE: TYPE: SOL; VALVE SIZE: 15 MM; TEMPERATURE RATING: MAX 160 DEG C; FACE TO FACE LENGTH: 130 MM; CONNECTION: FLANGE; OPERATED: ELECTRICAL; BODY MATERIAL: STAINLESS STEEL; OEM P/N: 12-EVDF 3R XN.W.U.P.09.29; SUPPL P/N: 799.010.010.0422; A2A50268347; 220 VDC","Uni Gerate","SOL","15 MM","STAINLESS STEEL",null,null,"FLANGE","130 MM",null,"ELECTRICAL",null,"MAX 160 DEG C"]
["0613741","VALVE: TYPE: NON RETURN,WAFER; VALVE SIZE: 54 MM; DESIGN RATING: 160 BAR; TEMPERATURE RATING: 300 DEG C; FACE TO FACE LENGTH: 25 MM; CONNECTION: COUPLING; OPERATED: PNEUMATIC; BODY MATERIAL: STAINLESS STEEL; STYLE: WAFER; TRIM: DISC SS; OEM P/N: A2A50005975; SUPPL P/N: 700.050.010.1028",null,"NON RETURN,WAFER","54 MM","STAINLESS STEEL","160 BAR","DISC SS","COUPLING","25 MM",null,"PNEUMATIC",null,"300 DEG C"]
["0622490","VALVE, SOLENOID: PIPE SIZE: DN25; STYLE: 1/2; POTENTIAL: 220 V; DESIGN RATING: PN40; CONNECTION: FLANGE; BODY MATERIAL: STEEL; OPERATED: ELECTRIC; ENCLOSURE RATING: IP65; MEDIUM: BUTANE/NATURAL GAS/PROPANE; CURRENT: 0.33 A; OEM P/N: A2A50272850; SUPPL P/N: PB0000267703",null,"SOLENOID","DN25","STEEL","PN40",null,"FLANGE",null,null,"ELECTRIC","BUTANE/NATURAL GAS/PROPANE"]
["0622492","VALVE, SOLENOID: PIPE SIZE: DN25; STYLE: 2/2; POTENTIAL: 230 V; DESIGN RATING: PN40; CONNECTION: FLANGE; BODY MATERIAL: STEEL; OPERATED: ELECTRIC; ENCLOSURE RATING: IP65; MEDIUM: BUTANE/NATURAL GAS/PROPANE; POWER: 160 W; CURRENT: 0.33 A; SPECIFICATION: DIN 3394-1; OEM P/N: 40-EVSADU 10NH-4 P.XN.09.20.32; SUPPL P/N: PB0000282466; A2A50296211","Uni Gerate","SOLENOID","DN25","STEEL","PN40",null,"FLANGE",null,null,"ELECTRIC","BUTANE/NATURAL GAS/PROPANE"]
["0626656","VALVE, CHECK: TYPE: HYDRAULIC; VALVE SIZE: G1/2 IN; DESIGN RATING: MAX 350 BAR; TEMPERATURE RATING: -30 TO 80 DEG C; CONNECTION: G1/2 IN-BSPP; BODY MATERIAL: STEEL; FACE TO FACE LENGTH: 16 MM; OPERATED: PNEUMATIC; OEM P/N: PG0031832800; SUPPL P/N: A2A50315038",null,"CHECK; HYDRAULIC","G1/2 IN","STEEL","MAX 350 BAR",null,"G1/2 IN-BSPP","16 MM",null,"PNEUMATIC",null,"-30 TO 80 DEG C"]
["0643634","VALVE: TYPE: CONTROL; VALVE SIZE: 6 IN; DESIGN RATING: 21 BAR; TEMPERATURE RATING: 65 DEG C; FACE TO FACE LENGTH: 235 MM; CONNECTION: WAFER; OPERATED: PILOT; BODY MATERIAL: CS; SPECIFICATION: 799-D; REFERENCE NO: 139163","INBAL","CONTROL","6 IN","CS","21 BAR",null,"WAFER","235 MM",null,"PILOT",null,"65 DEG C"]
["0644167","VALVE: TYPE: STOP; VALVE SIZE: DN 50; DESIGN RATING: 16 BAR; TEMPERATURE RATING: 120 DEG C; FACE TO FACE LENGTH: 150 MM; CONNECTION: FLANGE; OPERATED: MANUAL; BODY MATERIAL: CAST IRON; GRADE: EN-JL1040; SPECIFICATION: ARI 12072; .",null,"STOP","DN 50","CAST IRON","16 BAR",null,"FLANGE","150 MM",null,"MANUAL",null,"120 DEG C"]
["0644168","VALVE: TYPE: STOP; VALVE SIZE: DN 40; DESIGN RATING: 16 BAR; TEMPERATURE RATING: 120 DEG C; FACE TO FACE LENGTH: 140 MM; CONNECTION: FLANGE 150 MM; OPERATED: MANUAL; BODY MATERIAL: CAST IRON; GRADE: EN-JL1040; SPECIFICATION: ARI 12072",null,"STOP","DN 40","CAST IRON","16 BAR",null,"FLANGE 150 MM","140 MM",null,"MANUAL",null,"120 DEG C"]
["0644441","VALVE: TYPE: CONTROL; VALVE SIZE: 2 IN; DESIGN RATING: 21 BAR; TEMPERATURE RATING: 65 DEG C; FACE TO FACE LENGTH: 190 MM; CONNECTION: FLANGE; OPERATED: PILOT; BODY MATERIAL: CS; SPECIFICATION: 711-D","INBAL","CONTROL","2 IN","CS","21 BAR",null,"FLANGE","190 MM",null,"PILOT",null,"65 DEG C"]
["0644442","VALVE: TYPE: CONTROL; VALVE SIZE: 3 IN; DESIGN RATING: 21 BAR; TEMPERATURE RATING: 65 DEG C; FACE TO FACE LENGTH: 155 MM; CONNECTION: WAFER; OPERATED: PILOT; BODY MATERIAL: CARBON STL; SPECIFICATION: 799-D","INBAL","CONTROL","3 IN","CARBON STL","21 BAR",null,"WAFER","155 MM",null,"PILOT",null,"65 DEG C"]
["0644443","VALVE: TYPE: CONTROL; VALVE SIZE: 4 IN; DESIGN RATING: 21 BAR; TEMPERATURE RATING: 65 DEG C; FACE TO FACE LENGTH: 187 MM; CONNECTION: WAFER; OPERATED: PILOT; BODY MATERIAL: CARBON STL; SPECIFICATION: 799-D","INBAL","CONTROL","4 IN","CARBON STL","21 BAR",null,"WAFER","187 MM",null,"PILOT",null,"65 DEG C"]
["0647831","VALVE, BALL: VALVE SIZE: 1 IN; DESIGN RATING: 69 BAR; TEMPERATURE RATING: 50 DEG C; CONNECTION: BSP THREADED ENDS; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 88 MM; OPERATED: MANUAL; SOFTGOODS: PTFE; PORT TYPE: FULL BORE; GRADE: ASTM A351 GR CF8M; 2 PIECE SERIES 20",null,"BALL; FULL BORE","1 IN","STAINLESS STEEL","69 BAR",null,"BSP THREADED ENDS","88 MM",null,"MANUAL",null,"50 DEG C"]
["0647833","VALVE, BALL: VALVE SIZE: 3/4 IN; DESIGN RATING: 69; TEMPERATURE RATING: 50 DEG C; CONNECTION: BSP THREADED ENDS; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 74 MM; OPERATED: MANUAL; SOFTGOODS: PTFE; PORT TYPE: FULL BORE; GRADE: ASTM A351 GR CF8M; 2 PIECE SERIES 20",null,"BALL; FULL BORE","3/4 IN","STAINLESS STEEL","69",null,"BSP THREADED ENDS","74 MM",null,"MANUAL",null,"50 DEG C"]
["0650143","VALVE, SOLENOID: PIPE SIZE: 3/4 IN; STYLE: 9 X CONNECTIONS; 3 X SOLENOID; POTENTIAL: 24 VDC; DESIGN RATING: 3 BAR; CONNECTION: BSP; BODY MATERIAL: BRASS; OPERATED: DIRECT SOLENOID; ENCLOSURE RATING: IP67; MEDIUM: WATER; POWER: 11.2 W; ORIFICE SIZE: 19 MM; COIL: DC; APPLICATION: CENTRIFUGE SEALING WATER; CLASSIFICATION: ZONE 2; SUPPL P/N: 176346680","Alva-Laval","SOLENOID","3/4 IN; 19 MM","BRASS","3 BAR",null,"BSP",null,null,"DIRECT SOLENOID","WATER; CENTRIFUGE SEALING WATER"]
["0671840","VALVE, SOLENOID: PIPE SIZE: DN15; STYLE: BLOCK; POTENTIAL: 24 VDC; DESIGN RATING: 0.2-16 BAR; CONNECTION: PLUG; BODY MATERIAL: BRASS; OPERATED: DC V; ENCLOSURE RATING: IP65; MEDIUM: AIR/WATER; POWER: 11 W; CURRENT: 0.46 A; ORIFICE SIZE: 13 MM; SOFTGOODS: SEAL NBR; APPLICATION: GAS TURBINE FIRE SYSTEM; SPECIFICATION: ISO; MANUF P/N: 840131","Burkert","SOLENOID","DN15; 13 MM","BRASS","0.2-16 BAR",null,"PLUG",null,null,"DC V","AIR/WATER; GAS TURBINE FIRE SYSTEM"]
["0671894","VALVE: TYPE: CHANGE OVER; VALVE SIZE: 1-1/2 IN; DESIGN RATING: 40-100 BAR; TEMPERATURE RATING: -10 TO 425 DEG C; FACE TO FACE LENGTH: 265 MM; CONNECTION: DN 40; OPERATED: HAND; BODY MATERIAL: GP 240GM + N 1.0619; STYLE: CHANGE OVER VALVE; TRIM: CR 1,4021; GRADE: CARBON STEEL; SOFTGOODS: GRAPHITE/1,4571; SPECIAL FEATURES: CHANGE OVER VALVE,3 PORTS FLANGE; PN - 300 LBS","Leser","3 PORTS FLANGE; CHANGE OVER","1-1/2 IN","GP 240GM + N 1.0619","40-100 BAR","CR 1,4021","DN 40","265 MM",null,"HAND",null,"-10 TO 425 DEG C"]
["0708469","VALVE: TYPE: DELUGE; VALVE SIZE: 3 IN; DESIGN RATING: 21 BAR; TEMPERATURE RATING: 65 DEG C; CONNECTION: WAFER; OPERATED: ACTUATOR HYDRAULIC; BODY MATERIAL: FORGED STEEL SAE1021; INBAL MODEL 799DG-04-A01 HYDRAULIC DELGE VALVE- WAGER PATTERN ENDS RATED TO 21 TO OPEN WHEN PRESSURE IS LOST IN THE LINE, LATCH IN OPEN POSITION, LOCAL RESET COMPLETE WITH ALL NECESSARY TRIM VALVE ENDS AND WATER FLOW TEST & DRAIN ENDS DUCTILE (ASTM A53665-45-12), SLEEVE SMR5 ELATOMER REINFORCED WITH POLYESTER AND KEVLAR, CONTROL TRIM BRASS NICKEL CHROME PLATED STAINLESS STEEL AND GALVANISED STEEL","INBAL","DELUGE","3 IN","FORGED STEEL SAE1021","21 BAR",null,"WAFER",null,null,"ACTUATOR HYDRAULIC",null,"65 DEG C"]
["0708473","VALVE: TYPE: DELUGE; VALVE SIZE: 4 IN; DESIGN RATING: 21 BAR; TEMPERATURE RATING: 65 DEG C; CONNECTION: WAFER; OPERATED: ACTUATOR HYDRAULIC; BODY MATERIAL: FORGED STEEL SAE1021; INBAL MODEL 799DG-04-A01 HYDRAULIC DELGE VALVE- WAGER PATTERN ENDS RATED TO 21 TO OPEN WHEN PRESSURE IS LOST IN THE LINE, LATCH IN OPEN POSITION, LOCAL RESET COMPLETE WITH ALL NECESSARY TRIM VALVE ENDS AND WATER FLOW TEST & DRAIN ENDS DUCTILE (ASTM A53665-45-12), SLEEVE SMR5 ELATOMER REINFORCED WITH POLYESTER AND KEVLAR, CONTROL TRIM BRASS NICKEL CHROME PLATED STAINLESS STEEL AND GALVANISED STEEL","INBAL","DELUGE","4 IN","FORGED STEEL SAE1021","21 BAR",null,"WAFER",null,null,"ACTUATOR HYDRAULIC",null,"65 DEG C"]
["0713424","VALVE: TYPE: ISOLATING; VALVE SIZE: G1/2 IN; DESIGN RATING: 400 BAR; TEMPERATURE RATING: -20 TO 200 DEG C; FACE TO FACE LENGTH: 100 MM; CONNECTION: G1/2 IN; OPERATED: INSTRUMENT VALVE; BODY MATERIAL: STAINLESS STEEL; STYLE: VALVE WITH TEST PORT; TRIM: NEEDLE AND SEATING; GRADE: 1.4571; SPECIFICATION: DIN 16271; SOFTGOODS: CORROSION AND ACID RESISTANT; MANUF P/N: 9091157; SHUT-OFF VALVE WITH HEAT RESISTANT PLASTIC KNOB AND TEST PORT CONNECTION ,M20 X 1.5","WIKA","ISOLATING","G1/2 IN","STAINLESS STEEL","400 BAR","NEEDLE AND SEATING","G1/2 IN","100 MM",null,"INSTRUMENT VALVE",null,"-20 TO 200 DEG C"]
["0765058","VALVE: TYPE: RELIEF; VALVE SIZE: 25 MM; DESIGN RATING: 30 BAR; TEMPERATURE RATING: 170 DEG C; CONNECTION: FLANGE MM; OPERATED: SPRING; BODY MATERIAL: CARBON",null,"RELIEF","25 MM","CARBON","30 BAR",null,"FLANGE MM",null,null,"SPRING",null,"170 DEG C"]

{"sheet":"Drakensberg Pumped Storage","index":9,"n_rows":299,"n_cols":14,"rows_kept":299}
["Material","Original Description","OEM / Manufacturer","Valve Type","Size","Body Material","Class / Rating","Trim / Internals","End Connection","Face-to-Face","Drilling / PCD","Operation","Medium / Service","Medium Temperature"]
["0043262","VALVE: TYPE: SUCTION; VALVE SIZE: 144 MM; CONNECTION: COMPRESSION; OPERATED: PRESSURE; BODY MATERIAL: STAINLESS STEEL; TRIM: DISC STL; REFERENCE NO: HT303811; 2ND STAGE; 20P-4PORTS; 46.3MM THK PLATE; 88MM THK O/A; WITH HEX NUT, WASHER AND SPLIT PIN","HOWDEN","SUCTION","144 MM","STAINLESS STEEL","N/A","DISC STL","COMPRESSION","88 mm","N/S","PRESSURE","AIR","th"]
["0043264","VALVE: TYPE: SUCTION; VALVE SIZE: 104 MM; CONNECTION: COMPRESSION; OPERATED: PRESSURE; BODY MATERIAL: STAINLESS STEEL; TRIM: DISC STL; REFERENCE NO: HT303815; 4TH STAGE; 20P-2PORTS; 46.3MM THK PLATE; 89MM THK O/A; WITH HEX NUT, WASHER AND SPLIT PIN","Ariel Corporation/Howden","SUCTION","104 MM","STAINLESS STEEL","N/A","DISC STL","COMPRESSION","89 mm","N/S","PRESSURE","AIR","30-60 deg"]
["0043264","VALVE: TYPE: SUCTION; VALVE SIZE: 104 MM; CONNECTION: COMPRESSION; OPERATED: PRESSURE; BODY MATERIAL: STAINLESS STEEL; TRIM: DISC STL; REFERENCE NO: HT303815; 4TH STAGE; 20P-2PORTS; 46.3MM THK PLATE; 89MM THK O/A; WITH HEX NUT, WASHER AND SPLIT PIN","HOWDEN","SUCTION","104 MM","STAINLESS STEEL","N/A","DISC STL","COMPRESSION","90 mm","N/S","PRESSURE","AIR","40-80 deg"]
["0043264","VALVE: TYPE: SUCTION; VALVE SIZE: 104 MM; CONNECTION: COMPRESSION; OPERATED: PRESSURE; BODY MATERIAL: STAINLESS STEEL; TRIM: DISC STL; REFERENCE NO: HT303815; 4TH STAGE; 20P-2PORTS; 46.3MM THK PLATE; 89MM THK O/A; WITH HEX NUT, WASHER AND SPLIT PIN","HOWDEN/INGERSOL RAND","SUCTION","104 MM","STAINLESS STEEL","N/A","DISC STL","COMPRESSION","91 mm","N/S","PRESSURE","AIR","40-70 deg"]
["0043265","VALVE: TYPE: DISCHARGE; VALVE SIZE: 164 MM; CONNECTION: COMPRESSION; OPERATED: PRESSURE; BODY MATERIAL: STAINLESS STEEL; TRIM: DISC STL; REFERENCE NO: HT303810; ASSY; 1ST STAGE 20P- 5PORTS; 46.0MM THK PLATE; 70MM THK O/A; WITH HEX NUT AND SPLIT PIN","HOWDEN","DISCHARGE","164 MM","STAINLESS STEEL","N/A","DISC STL","COMPRESSION","92 mm","N/S","PRESSURE","AIR","100-180 deg"]
["0062413","VALVE, SOLENOID: PIPE SIZE: 12 MM; STYLE: 4 WAY; POTENTIAL: 240 - 250 VDC; DESIGN RATING: 70-700 KPA; CONNECTION: FNPT; BODY MATERIAL: BRASS; OPERATED: PRESSURE; ENCLOSURE RATING: IP65 EN 60529; MEDIUM: AIR/OIL/WATER; POWER: 11.2 W; APPLICATION: BLOWDOWN COMPRESSOR; REFERENCE NO: WP8345E001; GENERAL PURPOSE ENCLOSURE; 240 VDC COIL","ASCO / EMERSON","SOLENOID","12 MM","BRASS","70-700 KPA","N/S","FNPT","93 mm","N/S","PRESSURE","AIR/OIL/WATER; BLOWDOWN COMPRESSOR","90 deg"]
["0063152","VALVE, GATE: VALVE SIZE: 3/4 IN; TYPE: SOLID WEDGE; CONNECTION: FLANGE; BODY MATERIAL: BRASS; TRIM: DISC BRS; OPERATED: HANDWHEEL; STEM DESIGN: INSIDE SCREW; STYLE: THD BONNET; NEEDLE VALVE; FLANGE SIZE 105MM O/D; 4 HOLES 14MM DIA PCD 75MM; BS 2060","JONSON VALVE","GATE; SOLID WEDGE","3/4 IN","BRASS","BS 2060 (10 bar nominal pressure rating)","DISC BRS; INSIDE SCREW","FLANGE","94 mm","75MM; 4 HOLES 14MM DIA PCD 75MM","HANDWHEEL","water, air, fuel oil","0-100 DEG C"]
["0063348","VALVE, BALL: VALVE SIZE: 3/4 IN; DESIGN RATING: 1000 KPA; CONNECTION: FEMALE THD; OPERATED: LEVER; STYLE: 3 WAY; 3 PIECE; TRIM: BALL SS GR 316; SOFTGOODS: SEALS PTFE; GRADE: CF8M; ACID WATER OIL AND GAS; THROUGHWAY IN BALL TO BE 20 MM","SWAGELOK/PARKER HANNIFIN","BALL","3/4 IN","STEEL","1000 KPA","BALL SS GR 316","FEMALE THD","95 mm","N/S","LEVER","water, air, fuel oil","180 deg"]
["0065786","VALVE, GATE: VALVE SIZE: 250 MM; TYPE: SPHERICAL MANUAL BYPASS; CONNECTION: FLANGE; FACE TO FACE LENGTH: 250 MM; BODY MATERIAL: STEEL; OPERATED: HANDWHEEL; TEMPERATURE RATING: 16 DEG C; DESIGN RATING: 7.2 MPA; MAIN BY-PASS VALVE VOEST-ALPINE TYPE MB9-642-5320A ESKOM NO. 0.48/1121 DESIGNE PRESSURE = 7.2 MPA VALVE, BYPASS MAIN 5320 A","MB9-642-5320A","GATE; BYPASS MAIN 5320 A; SPHERICAL MANUAL BYPASS","250 MM","STEEL","7.2 MPA","N/S","FLANGE","96 mm","N/S","HANDWHEEL","water, air, fuel oil","16 DEG C"]
["0065917","VALVE, RELIEF: VALVE SIZE: 45 X 40 MM; SET PRESSURE: 70 BAR; CONNECTION: NPT X FNPT; BODY MATERIAL: STL; TRIM: DISC/SPRING STL; OPERATED: PRESSURE, SPRING; SAFETY","BAKER HUGHES/LASER","RELIEF","45 X 40 MM","STL","70 BAR","DISC/SPRING STL","NPT X FNPT","97 mm","N/S","PRESSURE, SPRING","water, air, fuel oil","oil 80-200 deg, air/gas 50-150"]
["0066072","VALVE, CHECK: TYPE: PISTON; VALVE SIZE: 25 MM; CONNECTION: NPT; BODY MATERIAL: STAINLESS STEEL; STYLE: THD CAP; TRIM: DISC/CAP STL; NON-RETURN; EO; TUBE SIZE 25MM OD EO TUBE CONNECTION AT BOTH ENDS","PARKER HANNIFIN/STAUFF","CHECK; PISTON","25 MM","STAINLESS STEEL","N/A","DISC/CAP STL","NPT","98 mm","N/S","Automatic flow operated","water, air, fuel oil","-200 TO 200 DEG C"]
["0066074","VALVE, BALL: VALVE SIZE: 16 MM; DESIGN RATING: 100 BAR; TEMPERATURE RATING: -200 TO 200 DEG C; CONNECTION: NPT X FNPT; BODY MATERIAL: STEEL; OPERATED: LEVER; STYLE: 4 WAY; TRIM: BALL STL; SPECIFICATION: DIN 3230; PORT TYPE: 3 X MALE; 1 X FEMALE; APPLICATION: UPSTREAM SEAL CHANGE OVER VALVE; TYPE: MANUAL OPERATED; SUPPL P/N: 1017489; REFERENCE NO: 1017489; 3 MALE X 1 FEMALE; CHANGE-OVER; BLOCK; ARGUS","Argus","BALL; 3 X MALE; MANUAL OPERATED","16 MM","STEEL","100 BAR","BALL STL","NPT X FNPT","99 mm","N/S","LEVER","UPSTREAM SEAL CHANGE OVER VALVE","-200 TO 200 DEG C"]
["0066205","VALVE, RELIEF: SET PRESSURE: 60 BAR; REFERENCE NO: MB8-222-2450C60B; SAFETY","MAXIMATOR GmbH","RELIEF","N/S","STEEL","60 BAR","Stainless Steel (SS), metal seated (hard-faced disc and nozzle).","TBC BY MANUFACTURE","100 mm","N/S","Pressure operated (automatic)","water, air, fuel oil","100 deg"]
["0066232","VALVE, DIAPHRAGM: VALVE SIZE: 15 MM; CONNECTION: FNPT; BODY MATERIAL: CI; DIAPHRAGM MATERIAL: RUBBER GR Q; OPERATED: HANDWHEEL; STYLE: WEIR; REFERENCE NO: A; SAUNDERS","Saunders","DIAPHRAGM","15 MM","CI; RUBBER GR Q","N/A","RUBBER GR Q","FNPT","101 mm","N/S","HANDWHEEL","water, air, fuel oil","0-80 deg"]
["0066529","VALVE, CHECK: TYPE: SWING; VALVE SIZE: 400 MM; DESIGN RATING: 16 BAR; CONNECTION: FLANGE; BODY MATERIAL: CS; TRIM: BONNET/DISC STEEL; REFERENCE NO: 16SMZ; CHECKRITE NON-RETURN; HYDRO. TEST CERTIFICATE REQUIRED FOR ALL VALVES","RITEPRO CORPORATION","CHECK; SWING","400 MM","CS","16 BAR","BONNET/DISC STEEL","FLANGE","102 mm","N/S","Automatic flow operated","N/S","100 deg"]
["0066535","VALVE, BALL: VALVE SIZE: 1/2 IN; DESIGN RATING: 40 LB; TEMPERATURE RATING: 25 DEG C; CONNECTION: FNPT; BODY MATERIAL: STAINLESS STEEL; OPERATED: LEVER; STYLE: UNION BONNET; TRIM: BALL SS; BRASS; WITH FIXED FEMALE FLANGE EITHER END","SWAGELOK/PARKER HANNIFIN","BALL","1/2 IN","STAINLESS STEEL","40 LB","BALL SS","FNPT","103 mm","N/S","LEVER","N/S","25 DEG C"]
["0068148","VALVE, RELIEF: VALVE SIZE: 50 MM; SET PRESSURE: 35 KPA; CONNECTION: THD; BODY MATERIAL: STL; TRIM: BRASS; OPERATED: SPRING; PRESSURE RANGE: 2-20 LB; REFERENCE NO: MD0014; SAFETY; TYPE 616-2; TYPE: HLP","MAXITROL","RELIEF; HLP","50 MM","STL","2-20 LB; 35 KPA","BRASS","THD","104 mm","N/S","SPRING","N/S","0-100 DEG C"]
["0070478","VALVE, RELIEF: VALVE SIZE: 50 X 32 MM; SET PRESSURE: 600 KPA; TEMPERATURE RATING: -10 TO 14 DEG C; CONNECTION: FLANGE; BODY MATERIAL: CI; TRIM: STAINLESS STEEL; OPERATED: PRESSURE; DESIGN RATING: 16 BAR; PRESSURE RANGE: 6 BAR; FIG NO: 4411/H2; REFERENCE NO: 16; SAFETY; INLET AND OUTLET PN16; TO SIZED TO DIN3320 AND TEST APPROVED IN ACCORDANCE WITH (AD-MERKBLATT A2); FLOW CAPACITY TO BE AT LEAST 35000 KG/HR","LESER","RELIEF","50 X 32 MM","CI","16 BAR; 6 BAR; 600 KPA","STAINLESS STEEL","FLANGE","105 mm","N/S","PRESSURE","N/S","-10 TO 14 DEG C"]
["0072012","VALVE, BALL: VALVE SIZE: 50 MM; DESIGN RATING: 6 BAR; CONNECTION: FLANGE; BODY MATERIAL: STEEL; OPERATED: LEVER; STYLE: 2 WAY; TRIM: BALL STL; BOHMER; SERIES FK","Bohmer","BALL","50 MM","STEEL","6 BAR","BALL STL","FLANGE","106 mm","N/S","LEVER","N/S","−20°C to 200 deg"]
["0072040","VALVE, GATE: VALVE SIZE: 3 IN; TYPE: SOLID WEDGE; CONNECTION: FLANGE; BODY MATERIAL: STEEL; TRIM: SEAT 13CR; OPERATED: HANDWHEEL; STEM DESIGN: RISING OUTSIDE SCREW; STYLE: BOLTED BONNET; GRADE: WCB; DESIGN RATING: 150 LB; REFERENCE NO: 2H27347; CAST; HIRATA","Hirata","GATE; SOLID WEDGE","3 IN","STEEL","150 LB","SEAT 13CR; RISING OUTSIDE SCREW","FLANGE","107 mm","N/S","HANDWHEEL","N/S","100 deg"]
["0072046","VALVE, GATE: VALVE SIZE: 2-1/2 IN; CONNECTION: FLANGE; BODY MATERIAL: CS; DESIGN RATING: 150 LB; DRAWING NO: 2H27346 REV 1","Flowserve","GATE","2-1/2 IN","CS","150 LB","13% Chromium Stainless Steel (AISI 410), hard-faced (CR13/HF)","FLANGE","108 mm","N/S","Manual gate operation","Water, Oil, Air","100 deg"]
["0072057","VALVE, GATE: VALVE SIZE: 100 MM; CONNECTION: FLANGE; BODY MATERIAL: CS; DESIGN RATING: 150 LB; REFERENCE NO: 2H27354; HIRATA","Hirata","GATE","100 MM","CS","150 LB","13Cr Stainless Steel (410 SS)","FLANGE","109 mm","N/S","Manual gate operation","Water, Oil, Air","−29°C to +425 deg"]
["0072058","VALVE, GATE: VALVE SIZE: 3/8 IN; TYPE: SOLID WEDGE; CONNECTION: FNPT; BODY MATERIAL: STEEL; TRIM: SEAT 13CR; OPERATED: HANDWHEEL; STEM DESIGN: RISING OUTSIDE SCREW; STYLE: BOLTED BONNET; DESIGN RATING: 600 LB; DRAWING NO: 2N27361 REV 1; FORGED; HIRATA","Hirata","GATE; SOLID WEDGE","3/8 IN","STEEL","600 LB","SEAT 13CR; RISING OUTSIDE SCREW","FNPT","110 mm","N/S","HANDWHEEL","Water, Oil, Air","−29°C to +425 deg"]
["0072060","VALVE, GLOBE: VALVE SIZE: 10 MM; OPERATED: HANDWHEEL; CONNECTION: FNPT; BODY MATERIAL: SS FORGED; TRIM: SEAT 13CR; STEM DESIGN: RISING OUTSIDE SCREW; STYLE: BOLTED BONNET; DESIGN RATING: 150 LB; DRAWING NO: 2S18670 REV 1; 3/8 INCH; HIRATA","Hirata","GLOBE","10 MM","SS FORGED","150 LB","SEAT 13CR; RISING OUTSIDE SCREW","FNPT","111 mm","N/S","HANDWHEEL","Water, Oil, Air","−29°C to +538 deg"]
["0072062","VALVE, GLOBE: VALVE SIZE: 1/2 IN; OPERATED: HANDWHEEL; CONNECTION: FLANGE; BODY MATERIAL: STL FORGED; TRIM: SEAT 13CR; STEM DESIGN: INSIDE SCREW; STYLE: BOLTED BONNET; DESIGN RATING: 150-800 LB; DRAWING NO: 2M18627 REV 1; HIRATA","Hirata","GLOBE","1/2 IN","STL FORGED","150-800 LB","SEAT 13CR; INSIDE SCREW","FLANGE","112 mm","N/S","HANDWHEEL","Water, Oil, Air","−29°C to +425 deg"]
["0073053","VALVE, BUTTERFLY: TYPE: WAFER; VALVE SIZE: 75 MM; DESIGN RATING: 740 LB; TEMPERATURE RATING: -250 TO 500 DEG F; CONNECTION: FLANGE; BODY MATERIAL: STAINLESS STEEL; TRIM: DISC SS GR 316; ELECTRICAL; MINITORK ASSY TURB","Minitork","BUTTERFLY; WAFER","75 MM","STAINLESS STEEL","740 LB","DISC SS GR 316","FLANGE","113 mm","N/S","Electrical actuator operated","Water, Oil, Air","-250 TO 500 DEG F"]
["0077118","VALVE, RELIEF: VALVE SIZE: 1/4 IN; SET PRESSURE: 60 LB; CONNECTION: NPT; BODY MATERIAL: BRASS; TRIM: SPRING STL; STEM BRS; OPERATED: PRESSURE, SPRING; SUPPL P/N: 3W123 662T2; STOP","Parker Hannifin","RELIEF","1/4 IN","BRASS","60 LB","SPRING STL","NPT","114 mm","N/S","PRESSURE, SPRING","Water, Oil, Air","−20°C to +200 deg"]
["0077124","VALVE: TYPE: DISCHARGE; VALVE SIZE: 27 MM; CONNECTION: COMPRESSION; OPERATED: PRESSURE; BODY MATERIAL: STL; TRIM: DISC STL; REFERENCE NO: 30279459","Burckhardt Compression","DISCHARGE","27 MM","STL","N/A","DISC STL","COMPRESSION","115 mm","N/S","PRESSURE","Water, Oil, Air","−29°C to +435 deg"]
["0077134","VALVE, RELIEF: VALVE SIZE: 1/4 IN; SET PRESSURE: 1300 LB; CONNECTION: NPT; BODY MATERIAL: BRASS; TRIM: SPRING STL; OPERATED: PRESSURE, SPRING; MODEL NO: 15T2; REFERENCE NO: X1396T19-1300; SAFETY; FOR TYPE 30; ING-RAND COMPRESSOR","Ing-Rand","RELIEF","1/4 IN","BRASS","1300 LB","SPRING STL","NPT","116 mm","N/S","PRESSURE, SPRING","Water, Oil, Air","120 deg"]
["0077142","VALVE, RELIEF: VALVE SIZE: 1/4 IN; SET PRESSURE: 1300 LB; CONNECTION: NPT; BODY MATERIAL: BRASS; TRIM: SPRING STL; STEM BRS; OPERATED: PRESSURE, SPRING; REFERENCE NO: W123662T2; SAFETY; ING-RAND","Ing-Rand","RELIEF","1/4 IN","BRASS","1300 LB","SPRING STL","NPT","117 mm","N/S","PRESSURE, SPRING","Water, Oil, Air","200 deg"]
["0077155","VALVE, SOLENOID: PIPE SIZE: 10 MM; STYLE: 5 WAY; POTENTIAL: 220 VAC; DESIGN RATING: 315 BAR; BODY MATERIAL: STEEL; MEDIUM: OIL; REFERENCE NO: S10G51G020001100; 35 HZ; CONNECTION MANIFOLD; GENERAL PURPOSE ENCLOSURE; PUMP PILOT VALVE","Bosch Rexroth","SOLENOID","10 MM","STEEL","315 BAR","N/S","Manifold mounted","118 mm","N/S","Solenoid operated","OIL","−20°C to +180 deg"]
["0077157","VALVE: TYPE: EXHAUST; VALVE SIZE: 15 MM; CONNECTION: THD FEMALE; OPERATED: PRESSURE; BODY MATERIAL: ALUMINIUM; STYLE: 3 WAY; TRIM: BONNET AL; REFERENCE NO: 3340 B 10 HD-D6461; SCHOVILL SCHREIDER QUICK SHUTTLE VALVES","Schrader Bellows","EXHAUST","15 MM","ALUMINIUM","N/A","BONNET AL","THD FEMALE","119 mm","N/S","PRESSURE","Water, Oil, Air","−20°C to +150 deg"]
["0077165","VALVE, BALL: VALVE SIZE: 25 MM; DESIGN RATING: 315 LB; CONNECTION: FNPT; BODY MATERIAL: STEEL; OPERATED: LEVER; STYLE: 2 WAY; BOHMER BLOCK","Bohmer","BALL","25 MM","STEEL","315 LB","Stainless Steel Ball / Reinforced PTFE Seats / Stainless Steel Stem","FNPT","120 mm","N/S","LEVER","Water, Oil, Air","−20°C to +250 deg"]
["0077169","VALVE, GATE: VALVE SIZE: 100 MM; TYPE: SOLID WEDGE; CONNECTION: FLANGE; BODY MATERIAL: STEEL; TRIM: BONNET STL; OPERATED: HYDRAULIC; STEM DESIGN: RISING OUTSIDE SCREW; STYLE: BOLTED BONNET; DESIGN RATING: 150 LB; REFERENCE NO: 20WRC; RUNNER COOLING WATER SUPPLY AUTO","Velan Inc.","GATE; SOLID WEDGE","100 MM","STEEL","150 LB","BONNET STL; RISING OUTSIDE SCREW","FLANGE","121 mm","N/S","HYDRAULIC","Water, Oil, Air","up to 60 deg"]
["0077200","VALVE: TYPE: SUCTION; VALVE SIZE: 167 MM; CONNECTION: COMPRESSION; OPERATED: PRESSURE; BODY MATERIAL: STL; TRIM: DISC STL; REFERENCE NO: HT303809; 1ST STAGE","Burckhardt Compression","SUCTION","167 MM","STL","N/A","DISC STL","COMPRESSION","122 mm","N/S","PRESSURE","Water, Oil, Air","up to 50 deg"]
["0077201","VALVE: TYPE: DISCHARGE; VALVE SIZE: 145 MM; CONNECTION: COMPRESSION; OPERATED: PRESSURE; BODY MATERIAL: STL; TRIM: DISC STL; REFERENCE NO: HT303812; ASSEMBLY; 2ND STAGE","Burckhardt Compression","DISCHARGE","145 MM","STL","N/A","DISC STL","COMPRESSION","123 mm","N/S","PRESSURE","Water, Oil, Air","up to 180 deg"]
["0077202","VALVE: TYPE: DISCHARGE; VALVE SIZE: 103.7 MM; DESIGN RATING: 0-250 DEG C; TEMPERATURE RATING: 0-250 DEG C; CONNECTION: COMPRESSION; OPERATED: PRESSURE; BODY MATERIAL: STL; TRIM: DISC STL; REFERENCE NO: HT303814; ASSEMBLY; 3RD STAGE","Burckhardt Compression","DISCHARGE","103.7 MM","STL","0-250 DEG C","DISC STL","COMPRESSION","124 mm","N/S","PRESSURE","Water, Oil, Air","0-250 DEG C"]
["0077203","VALVE: TYPE: DISCHARGE; VALVE SIZE: 104.4 MM; CONNECTION: COMPRESSION; OPERATED: PRESSURE; BODY MATERIAL: STL; TRIM: DISC STL; REFERENCE NO: HT303816; ASSEMBLY; 4TH STAGE","Burckhardt Compression","DISCHARGE","104.4 MM","STL","N/A","DISC STL","COMPRESSION","125 mm","N/S","PRESSURE","Water, Oil, Air","150-220 deg"]
["0077242","VALVE, ANGLE: TYPE: GLOBE; VALVE SIZE: 100 MM; DESIGN RATING: 600 LB; CONNECTION: FLANGE; BODY MATERIAL: STL; OPERATED: HYDRAULIC; STYLE: BOLTED BONNET; TRIM: BONNET/STEM STL; DRAWING NO: M-6WO78AG8 REV 1; REFERENCE NO: 20DA1/2; AIR ADMISSION; FOR TAIL WATER DEPRESSING","Velan Inc.","ANGLE; GLOBE","100 MM","STL","600 LB","BONNET/STEM STL","FLANGE","126 mm","N/S","HYDRAULIC","Water, Oil, Air","5-40 deg"]
["0178035","VALVE, RELIEF: REFERENCE NO: 0523C","Maxitrol Company/Baker Hughes","RELIEF","N/S","STEEL","N/A","N/S","TBC","127 mm","N/S","Pressure operated (automatic)","Water, Oil, Air","20-120 deg"]
["0401291","VALVE, BALL: VALVE SIZE: 3/4 IN; OPERATED: HANDLE; TYPE: STOP","Parker Hannifin/KITZ Corporation","BALL; STOP","3/4 IN","STEAL","10-40 BAR","BALL STL","TBC","128 mm","N/S","HANDLE","Water, Oil, Air","−20 to +180 deg"]
["0403617","VALVE, RELIEF: APPLICATION: LATCO PRESSURE CONTROL; DESIGN RATING: 400 KPA","LATCO","RELIEF","N/S","STEEL","400 KPA","N/S","TBC","129 mm","N/S","Pressure operated (automatic)","LATCO PRESSURE CONTROL","20-80 deg"]
["0502387","VALVE: TYPE: COMPRESSOR 3RD STAGE; OPERATED: AUTOMATIC; BODY MATERIAL: STL; SUPPL P/N: 31517725","Burckhardt Compression","COMPRESSOR 3RD STAGE","N/S","STL","N/A","Concentric Ring Valve – Hardened Steel / Stainless Steel","TBC","130 mm","N/S","AUTOMATIC","AIR","−29°C to +425 deg"]
["0502388","VALVE: TYPE: COMPRESSOR 2ND STAGE; OPERATED: AUTOMATIC; BODY MATERIAL: STL; SUPPL P/N: 37004827","Burckhardt Compression","COMPRESSOR 2ND STAGE","N/S","STL","N/A","Concentric ring valve assembly comprising hardened alloy steel seat, stainless steel valve plates (rings), and spring steel springs.","TBC","131 mm","N/S","AUTOMATIC","AIR","−29°C to +425 deg"]
["0502396","VALVE: TYPE: 1ST STAGE; VALVE SIZE: 164MM X 85 IN; TEMPERATURE RATING: 0-250 DEG C; CONNECTION: COMPRESSION; OPERATED: AUTOMATIC; BODY MATERIAL: STEEL; MANUF P/N: 37101946","Burckhardt Compression","1ST STAGE","164MM X 85 IN","STEEL","N/A","N/S","COMPRESSION","132 mm","N/S","AUTOMATIC","AIR","0-250 DEG C"]
["0640478","VALVE, GLOBE: VALVE SIZE: 2 IN; DESIGN PRESSURE: 102 BAR; DESIGN TEMPERATURE: -29 TO 38 DEG C; FACE TO FACE LENGTH: 292.1 MM; OPERATED: HANDWHEEL, MANUAL; CONNECTION: FLANGE; BODY MATERIAL: A216 GR WCB; TRIM: A182F6; GRADE: A216 GR WCB; SOFTGOODS: PACKING GRAPHITE; STEM DESIGN: A182F6; APPLICATION: RUNNER SEAL ISOLATION; SPECIFICATION: CL 600; TYPE: ISOLATING; DESIGN RATING: ASME B19.34; TEMPERATURE RATING: ASME B16.34; CONNECTION ASME B16.5/B16.25; TESTING AND INSPECTION; API 598","Velan Inc.","GLOBE; ISOLATING","2 IN","A216 GR WCB","ASME B19.34; 102 BAR","A182F6","FLANGE","133 mm","N/S","HANDWHEEL, MANUAL","RUNNER SEAL ISOLATION","ASME B16.34; -29 TO 38 DEG C"]
["0640479","VALVE, BUTTERFLY: TYPE: DRAIN WAFER; VALVE SIZE: DN 32; DESIGN RATING: PN25; TEMPERATURE RATING: NBR -10 TO 90 DEG C; CONNECTION: FLANGE; BODY MATERIAL: 2EN-GJS-4000-15(GGG-40) EPOXY COATED 120 UM; FACE TO FACE LENGTH: 33 MM; OPERATED: ACTUATOR PNEUMATIC; TRIM: A1.4408 INVESTMENT CASTING; SOFTGOODS: NBR; APPLICATION: SHAFT/RUNNER SEAL DRAIN; GRADE: DN 25-600; SPECIFICATION: D480; SCHEDULE: ASME B16.47; SERIES A; CL 150; SPECIAL FEATURES: BARE SHAFT; SUPPL P/N: D480 32W332A1NLF07 D11; CONNECTION TYPE; 3EN1092 PN16, OPERATING PRESSUE; 3.16 BAR, SHAFT MATERIAL; 1AISI420/1.4021, SHAFT LENGTH; 18, 18 MM, SEAT LINER; N NBR","EBRO Armaturen","BUTTERFLY; DRAIN WAFER","DN 32","2EN-GJS-4000-15(GGG-40) EPOXY COATED 120 UM","PN25","A1.4408 INVESTMENT CASTING","FLANGE","134 mm","N/S","ACTUATOR PNEUMATIC","SHAFT/RUNNER SEAL DRAIN","NBR -10 TO 90 DEG C"]
["0777978","VALVE, SOLENOID: PIPE SIZE: 10 MM; STYLE: 4 PIPE CONNECTION 2 SOLENOID; POTENTIAL: 24 VDC; DESIGN RATING: 16 BAR; CONNECTION: 10 MM; BODY MATERIAL: ALUMININIUM; OPERATED: 24 V DC; ENCLOSURE RATING: 16 BAR; MEDIUM: AIR PNEUMATIC; OEM P/N: MPZWIDC.124 (0065745.002); PNEUMATIC CONTROL BLOCK, TYPE:MPZWIDC.124, ON WALL OR IN CABINET MOUNT, 2.5 KG, TWO CONTROL SOLENOIDS","Festo","SOLENOID; MPZWIDC.124, ON WALL OR IN CABINET MOUNT, 2.5 KG, TWO CONTROL SOLENOIDS","10 MM","ALUMINIUM","16 BAR","Stainless steel spool and armature with NBR (Buna-N) seals.","10 MM","95 mm","N/S","24 V DC","AIR PNEUMATIC","5°C to 39 deg"]
["0654743","VALVE, BALL: VALVE SIZE: 1/2 IN; APPLICATION: AMMONIA SOLUTION LINE TO FEEDWATER TANK; TYPE: QUICK STOP; SUPPL P/N: N300","Nupro (Swagelok)","BALL; QUICK STOP","1/2 IN","STEEL","27.6 BAR","SS316 ball and stem with PTFE seats and seals.","TBC","2NIA SOLUTION / Internals, End Connection, Face-to-Face, Drilling / Internals, End Connection, Face-to-Face, Drilling","N/S","MANUAL","AMMONIA SOLUTION LINE TO FEEDWATER TANK","10°C to 40 deg"]
["0662552","VALVE, CHECK: TYPE: NON RETURN; VALVE SIZE: 80 MM; DESIGN RATING: PN40; TEMPERATURE RATING: 50 DEG C; CONNECTION: BW; BODY MATERIAL: CI; FACE TO FACE LENGTH: 173 MM; OPERATED: AUTOMATIC; TRIM: STL; APPLICATION: LIMESTONE HYDRAULIC FEEDER DRIVE; SPECIFICATION: TH-CD-2572-00-02; SUPPL P/N: 2572-00-02-14","KSB","CHECK; NON RETURN","80 MM","CI","PN40","STL","BW","173 MM","N/S","AUTOMATIC","LIMESTONE HYDRAULIC FEEDER DRIVE","50 DEG C"]
["0662572","VALVE, CHECK: TYPE: NON RETURN; VALVE SIZE: 100 MM; DESIGN RATING: PN25; TEMPERATURE RATING: 55 DEG C; CONNECTION: BW; BODY MATERIAL: CAST STL; FACE TO FACE LENGTH: 170 MM; OPERATED: FLOW; TRIM: STL; APPLICATION: LIMESTONE HYDRAULIC FEEDER DRIVE; SPECIFICATION: TH-CD-2572-00-02; SUPPL P/N: 2572-00-02-25","KSB","CHECK; NON RETURN","100 MM","CAST STL","PN25","STL","BW","170 MM","N/S","FLOW","LIMESTONE HYDRAULIC FEEDER DRIVE","55 DEG C"]
["0696638","VALVE, BUTTERFLY: TYPE: CENTERED DISC; VALVE SIZE: 3 IN; DESIGN RATING: PN35; TEMPERATURE RATING: 0-100 DEG C; CONNECTION: BW; BODY MATERIAL: 1.4571; FACE TO FACE LENGTH: 400 MM; OPERATED: MANUAL; TRIM: STL; SOFTGOODS: GASKETS; APPLICATION: DRAIN VALVE 1 TURBINE HOUSE UNIT 4; 4 0LCE10 AA401; SPECIFICATION: AV-25-63-SE-HR-G-XX-00; SUPPL P/N: 63906F3C7C3F09C3E0401EAC37FA0A05","ANDRITZ","BUTTERFLY; CENTERED DISC","3 IN",1.4571,"PN35","STL","BW","400 MM","N/S","MANUAL","DRAIN VALVE 1 TURBINE HOUSE UNIT 4","0-100 DEG C"]
["0738822","VALVE: TYPE: INJECTION; VALVE SIZE: 6/4 - R 1/2 IN; DESIGN RATING: 7-16 BAR; TEMPERATURE RATING: 25-40 DEG; CONNECTION: 6 MM COMPRESSION; OPERATED: STANDARD; BODY MATERIAL: PVC; .","ProMinent","INJECTION","6/4 - R 1/2 IN","PVC","7-16 BAR","PTFE seat with ceramic (or SS316) ball, Hastelloy C/SS316 spring, and EPDM seals.","6 MM COMPRESSION","INJECTION; VALVE SIZE: 6/4 - R 104 s, Face-to-Face, Drilling / PCD, Mediums, Face-to-Face, Drilling / PCD, Medium","N/S","STANDARD","Water treatment chemicals/Chemical dosing/injection systems","25-40 DEG"]
["0738824","VALVE: TYPE: FOOT; VALVE SIZE: 20 MM; DESIGN RATING: 7-16 BAR; TEMPERATURE RATING: 40 DEG; CONNECTION: 6 MM COMPRESSION; OPERATED: STANDARD; BODY MATERIAL: PVDF PTFE","ProMinent","FOOT","20 MM","PVDF PTFE","7-16 BAR","Ceramic ball, PTFE seat, Hastelloy C spring (where applicable), PTFE/FKM seals.","6 MM COMPRESSION","FOOT; VALVE SIZE: 2001 s, Face-to-Face, Drilling / PCD, Mediums, Face-to-Face, Drilling / PCD, Medium","N/S","STANDARD","Water treatment chemicals/Chemical dosing/injection systems","40 DEG"]
["0754488","VALVE, SOLENOID: PIPE SIZE: G1/2 Thread ACRE; STYLE: 2/2-WAYS, NORMALLY CLOSED; POTENTIAL: 24 VDC; DESIGN RATING: PN 80 BAR; CONNECTION: GM84 - G1/2 THREADED PORT; BODY MATERIAL: MS BRASS; OPERATED: VOLTAGE; ENCLOSURE RATING: IP65; MEDIUM: WATER. AIR AND HYDRAULIC FLUIDS; POWER: 24 VDC; SUPPL P/N: 5404-A12,0EFMSGM84-C024/DC-12; BURKERT: 2/2-WAY-SOLENOID VALVE; SERVO-POSITION, 5404-A12,0EFMSGM84-C024/DC-12 A 2/2-WAYS;NORMALY CLOSED, ORIFICE SIZE - EF PTFE-SEAT-SEALING + FKM, MATERIAL - MS BRASS, PORT CONNECTION - GM84 G1/2 THREADED PORT, COIL SIZE - C 40 X 40, VOLTAGE - 024 24VOLTS, FREQUENCY - DC, POWER CONSUMPTION - 12 WATT, SPECIAL FEATURE MX13 PN 80 BAR RATED","Burkert","SOLENOID","G1/2 Thread ACRE","MS BRASS","PN 80 BAR","Stainless steel internals with PTFE seat and FKM (Viton) seal.","GM84 - G1/2 THREADED PORT; GM84 G1/2 THREADED PORT","95 acre","N/S","VOLTAGE","WATER. AIR AND HYDRAULIC FLUIDS","up to 200 deg"]
["0042716","BODY: TYPE: PILOT VALVE; DIMENSIONS: DIA 15.5 X LG 36.4 MM; MATERIAL: BRASS; MODEL NO: 41; REFERENCE NO: 3W63625 T30; COMP; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Parker Hannifin","PILOT VALVE","36.4 MM","BRASS","150-600 Psi","Stainless steel internals with NBR/PTFE seat and stainless steel spring.","TBC","A2 x lg 36.4 mm","N/S","PRESSURE","Pilot Valve","up to 200 deg"]
["0041833","VALVE: TYPE: COMPRESSOR; VALVE SIZE: 175 MM; OPERATED: PRESSURE; BODY MATERIAL: STL; TRIM: DISC SS; 2ND STAGE CONCENTRIC","Burckhardt Compression","COMPRESSOR","175 MM","STL","150-600 Psi","DISC SS","TBC","95 mm","N/S","PRESSURE","Compressor","40-80 deg"]
["0041913","ASSEMBLY: TYPE: PILOT VALVE; SUPPL P/N: R53608T10; REFERENCE NO: 10-11; COMPLETE; FOR DIESEL GENERATOR AIR STATOR COMPRESSOR; INGERSOLL RAND TYPE 30 MODEL 41","INGERSOLL RAND TYPE 30; Ingersoll Rand","PILOT VALVE","N/S","STMBLY:","10 BAR","N/S","TBC","70 mm","N/S","PRESSURE","Pilot Valve","20-80 deg"]
["0043215","VALVE: VALVE SIZE: 68 MM; CONNECTION: COMPRESSION; OPERATED: PRESSURE; BODY MATERIAL: STL; TRIM: DISC STL; SUPPL P/N: 22K1R; REFERENCE NO: 30220479; COMPLETE; FOR TYPE 30 MODEL 41 ING-RAND AIR COMPRESSOR; SIZE 25.5MM THK","FOR TYPE 30; Ing-Rand","Compressor valve","68 MM","STL","N/A","DISC STL","COMPRESSION","3Ponnection: compression; operated: pressure; body material: stl; trim: disc stl","N/S","PRESSURE","AIR/OIL/WATER;","TBC"]
["0043216","VALVE: TYPE: DISCHARGE; VALVE SIZE: 68 MM; CONNECTION: COMPRESSION; OPERATED: PRESSURE; BODY MATERIAL: STL; TRIM: DISC STL; SUPPL P/N: CPN 30217947; REFERENCE NO: 30217947; 22K2R; SIZE 26.4MM THK; COMPLETE; FOR TYPE 30 MODEL 41 ING- RAND AIR COMPRESSOR","FOR TYPE 30","DISCHARGE","68 MM","STL","N/A","DISC STL","COMPRESSION","ENCE NO: 30217947; 22ENCE NO: 30217947; 22 ing / PCD, Mediuming / PCD, Medium","N/S","PRESSURE","AIR/OIL/WATER;","TBC"]
["0043234","KIT, COMPRESSOR REPAIR: TYPE: TUNE UP/RING/VALVE; MODEL NO: 15T2; REFERENCE NO: 32226342; 32133951; FOR TYPE 30 COMPRESSOR","Ingersoll Rand","TUNE UP/RING/VALVE","Not specified","Not specified","N/A","Cast iron piston rings, stainless steel valve plates, hardened steel seats, spring steel springs, NBR/PTFE seals and fiber gaskets.","COMPRESSION","R3 ring/valve; model no: 15t2","N/S","PRESSURE","N/A","N/A"]
["0043262","VALVE: TYPE: SUCTION; VALVE SIZE: 144 MM; CONNECTION: COMPRESSION; OPERATED: PRESSURE; BODY MATERIAL: STAINLESS STEEL; TRIM: DISC STL; REFERENCE NO: HT303811; 2ND STAGE; 20P-4PORTS; 46.3MM THK PLATE; 88MM THK O/A; WITH HEX NUT, WASHER AND SPLIT PIN","Burckhardt Compression","SUCTION","144 MM","STAINLESS STEEL","150-600 Psi","DISC STL","COMPRESSION","3T size: 144 mm; connection: compression; operated: pressure; body material: stainless steel; trim: disc stl; reference no: ht303811","N/S","PRESSURE","AIR/OIL/WATER;","−196 to +538 deg"]
["0043263","VALVE: TYPE: SUCTION; VALVE SIZE: 104 MM; CONNECTION: COMPRESSION; OPERATED: PRESSURE; BODY MATERIAL: STL; STYLE: 2 PORT; TRIM: DISC STL; REFERENCE NO: HT303813; ASSY; 3RD STAGE 20P-2PORTS; 104MM DIA; 44.3MM THK PLATE; 88MM THK O/A; WITH HEX NUT; WASHER AND SPLIT PIN","Burckhardt Compression","SUCTION","104 MM","STL","N/A","DISC STL","COMPRESSION","95 mm","N/S","PRESSURE","AIR/OIL/WATER;","up to 100 deg"]
["0042019","VALVE: VALVE SIZE: 10 MM; CONNECTION: COMPRESSION; OPERATED: PRESSURE; BODY MATERIAL: STL; STYLE: 5 WAY; TRIM: BONNET STL; REFERENCE NO: TC2G0340; THROTTLE AND CHECK MODULE","Hoerbiger","CHECK","10 MM","STL","N/A","BONNET STL","COMPRESSION","2Nonnection: compression; operated: pressure","N/S","PRESSURE","AIR/OIL/WATER;","up to 425 deg"]
["0042712","CAP: TYPE: VALVE CAGE; DIMENSIONS: DIA 39 X HT 22 MM; MATERIAL: STL; REFERENCE NO: 3W75338; FOR 8K AIR HEAD ASSEMBLY; TYPE 30 MODEL 41 ING- RAND AIR COMPRESSOR","TYPE 30","VALVE CAGE","39 MM","STL","N/A","Steel valve cage with spring stainless steel valve plate, hardened steel seat, and spring steel spring assembly.","COMPRESSION","22 mm","N/S","PRESSURE","AIR/OIL/WATER;","up to 200 deg"]
["0043264","VALVE: TYPE: SUCTION; VALVE SIZE: 104 MM; CONNECTION: COMPRESSION; OPERATED: PRESSURE; BODY MATERIAL: STAINLESS STEEL; TRIM: DISC STL; REFERENCE NO: HT303815; 4TH STAGE; 20P-2PORTS; 46.3MM THK PLATE; 89MM THK O/A; WITH HEX NUT, WASHER AND SPLIT PIN","Burckhardt Compression","SUCTION","104 MM","STAINLESS STEEL","N/A","DISC STL","COMPRESSION","3T size: 104 mm; connection: compression; operated: pressure; body material: stainless steel; trim: disc stl; reference no: ht303815","N/S","PRESSURE","AIR/OIL/WATER;","up to 120 deg"]
["0043265","VALVE: TYPE: DISCHARGE; VALVE SIZE: 164 MM; CONNECTION: COMPRESSION; OPERATED: PRESSURE; BODY MATERIAL: STAINLESS STEEL; TRIM: DISC STL; REFERENCE NO: HT303810; ASSY; 1ST STAGE 20P- 5PORTS; 46.0MM THK PLATE; 70MM THK O/A; WITH HEX NUT AND SPLIT PIN","Burckhardt Compression","DISCHARGE","164 MM","STAINLESS STEEL","N/A","DISC STL","COMPRESSION","3 ve size: 164 mm; connection: compression; operated: pressure; body material: stainless steel; trim: disc stl; reference no: ht303810","N/S","PRESSURE","AIR/OIL/WATER;","80-120 deg"]
["0043268","VALVE: TYPE: DISCHARGE; REFERENCE NO: HT303799; 34-00; 2ND STAGE; RETAINER ASSY","Burckhardt Compression","DISCHARGE","N/S","STEYP","N/A","Steel retainer with stainless steel valve plate, hardened steel seat and stop plate, spring steel springs.","COMPRESSION","N/S","N/S","PRESSURE","AIR/OIL/WATER;","100-160 deg"]
["0043269","VALVE: TYPE: SUCTION; DRAWING NO: HT 303857 REV 1; REFERENCE NO: 35-00; 3RD STAGE; RETAINER ASSY","Burckhardt Compression","SUCTION","N/S","STEYP","N/A","Steel retainer assembly with stainless steel suction valve plate, hardened steel seat and stop plate, spring steel springs.","COMPRESSION","N/S","N/S","PRESSURE","AIR/OIL/WATER;","40-80 deg"]
["0043270","VALVE: TYPE: DISCHARGE; REFERENCE NO: HT303800; 36-00; 3RD STAGE; RETAINER ASSY","Burckhardt Compression","DISCHARGE","N/S","STEYP","N/A","Steel retainer assembly with stainless steel discharge valve plate, hardened steel seat and stop plate, spring steel springs.","COMPRESSION","N/S","N/S","PRESSURE","AIR/OIL/WATER;","up to 150"]
["0043271","VALVE: TYPE: SUCTION; REFERENCE NO: 37-00; HT303858; 4TH STAGE; RETAINER ASSY","Burckhardt Compression","SUCTION","N/S","STEYP","N/A","Steel retainer assembly with stainless steel suction valve plate, hardened steel seat and stop plate, spring steel springs.","COMPRESSION","N/S","N/S","PRESSURE","AIR/OIL/WATER;","up to 120 deg"]
["0062413","VALVE, SOLENOID: PIPE SIZE: 12 MM; STYLE: 4 WAY; POTENTIAL: 240 - 250 VDC; DESIGN RATING: 70-700 KPA; CONNECTION: FNPT; BODY MATERIAL: BRASS; OPERATED: PRESSURE; ENCLOSURE RATING: IP65 EN 60529; MEDIUM: AIR/OIL/WATER; POWER: 11.2 W; APPLICATION: BLOWDOWN COMPRESSOR; REFERENCE NO: WP8345E001; GENERAL PURPOSE ENCLOSURE; 240 VDC COIL","ASCO Numatics","SOLENOID","12 MM","BRASS","70-700 KPA","SS spool & armature with NBR seals and PTFE guide rings","FNPT","95 mm","N/S","PRESSURE","AIR/OIL/WATER; BLOWDOWN COMPRESSOR","80 deg"]
["0044480","CONTROL: TYPE: PUMP VALVE ASSY","Burckhardt Compression/Ingersoll Rand/KSB","PUMP VALVE ASSY","N/S","Not specified","N/A","Hardened steel spool/poppet with hardened seat, spring steel spring, and NBR/PTFE sealing system.","TBC","N/S","N/S","TBC","TBC","TBC"]
["0061543","ADAPTOR: TYPE: PILOT VALVE; MATERIAL: BRASS; REFERENCE NO: 3W39895; FOR TYPE 30 MODEL 15T2 ING-RAND AIR COMPRESSOR; SIZE 20MM DIA X 60MM LG","FOR TYPE 30; Ing-Rand","PILOT VALVE","20 MM","BRASS","N/A","Brass body with NBR seals and PTFE guide/seal elements","pilot valve assembly",";1 reference","N/S","pilot valve assembly","AIR","up to 200 deg"]
["0062540","VALVE, SOLENOID: POTENTIAL: 220 V; SUPPL P/N: S2155","ASCO Numatics/Parker Hannifin/Festo","SOLENOID","N/S","STEOL","N/A","Stainless steel plunger and core with NBR seals and brass/stainless seat.","TBC","N/S","N/S","Electrically actuated valve","GAS/LIQUID","TBC"]
["0062568","VALVE, SOLENOID: PIPE SIZE: 10 MM; STYLE: 2 WAY; POTENTIAL: 220 VDC; DESIGN RATING: 100 BAR; CONNECTION: FNPT; BODY MATERIAL: BRASS; OPERATED: NC; ENCLOSURE RATING: IP65; MEDIUM: GAS/LIQUID; POWER: 16 W; REFERENCE NO: 9107500/0701","Burkert","SOLENOID","10 MM","BRASS","100 BAR","Stainless steel plunger and core with PTFE guide rings, FKM/NBR seals, and brass/stainless seat system.","FNPT","5OTENTIAL: 220 VDC; DESIGN RATING: 100 llinglling","N/S","NC","GAS/LIQUID","up to 200 deg"]
["0063087","VALVE, SOLENOID: PIPE SIZE: 10 MM; STYLE: 5 WAY; BODY MATERIAL: STEEL; OPERATED: DOUBLE ACTING; MEDIUM: LIQUID; YUKEN; ENCLOSURE: GENERAL PURPOSE; CONNECTION MANIFOLD","Yuken Kogyo","SOLENOID","10 MM","STEEL","N/A","Stainless steel plunger and core with PTFE guide rings, FKM/NBR seals, and hardened brass/stainless seat system.","Manifold mounted","95 mm","N/S","DOUBLE ACTING","LIQUID","−29 to +425 deg"]
["0063152","VALVE, GATE: VALVE SIZE: 3/4 IN; TYPE: SOLID WEDGE; CONNECTION: FLANGE; BODY MATERIAL: BRASS; TRIM: DISC BRS; OPERATED: HANDWHEEL; STEM DESIGN: INSIDE SCREW; STYLE: THD BONNET; NEEDLE VALVE; FLANGE SIZE 105MM O/D; 4 HOLES 14MM DIA PCD 75MM; BS 2060","Bristol Valves","GATE; SOLID WEDGE","3/4 IN","BRASS","N/A","DISC BRS; INSIDE SCREW","FLANGE","5; mm","75MM; 4 HOLES 14MM DIA PCD 75MM","HANDWHEEL","AIR/OIL/WATER;","up to 200 deg"]
["0065785","VALVE: TYPE: IMPULSE; VALVE SIZE: 15 MM; CONNECTION: THD FEMALE; OPERATED: PRESSURE; BODY MATERIAL: STL; TRIM: DISC STL; DRAWING NO: MB9-642.6350B REV 1; MANIFOLD; SIZE 18MM THK","Burckhardt Compression","IMPULSE","15 MM","STL","N/A","DISC STL","THD FEMALE","5S size: 15 mm; connection: thd female; operated: pressure","N/S","PRESSURE","TBC","TBC"]
["0065786","VALVE, GATE: VALVE SIZE: 250 MM; TYPE: SPHERICAL MANUAL BYPASS; CONNECTION: FLANGE; FACE TO FACE LENGTH: 250 MM; BODY MATERIAL: STEEL; OPERATED: HANDWHEEL; TEMPERATURE RATING: 16 DEG C; DESIGN RATING: 7.2 MPA; MAIN BY-PASS VALVE VOEST-ALPINE TYPE MB9-642-5320A ESKOM NO. 0.48/1121 DESIGNE PRESSURE = 7.2 MPA VALVE, BYPASS MAIN 5320 A","MB9-642-5320A","GATE; BYPASS MAIN 5320 A; SPHERICAL MANUAL BYPASS","250 MM","STEEL","7.2 MPA","13Cr/Alloy steel spherical wedge, Stellite hard-faced seats, SS stem, graphite packing","FLANGE","250 MM","N/S","HANDWHEEL","WATER","16 DEG C"]
["0063285","VALVE, RELIEF: VALVE SIZE: 12 MM; CONNECTION: FNPT; BODY MATERIAL: STL; TRIM: SPRING STL; OPERATED: PRESSURE; REFERENCE NO: M67E; HP UNIT PILOT; DAIKIN","Daikin Industries","RELIEF","12 MM","STL","N/A","SPRING STL","FNPT","3E12 mm","N/S","PRESSURE","AIR,WATER,OIL","−29 to +425 deg"]
["0063348","VALVE, BALL: VALVE SIZE: 3/4 IN; DESIGN RATING: 1000 KPA; CONNECTION: FEMALE THD; OPERATED: LEVER; STYLE: 3 WAY; 3 PIECE; TRIM: BALL SS GR 316; SOFTGOODS: SEALS PTFE; GRADE: CF8M; ACID WATER OIL AND GAS; THROUGHWAY IN BALL TO BE 20 MM","Parker Hannifin","BALL","3/4 IN","MEEAL","1000 KPA","BALL SS GR 316","FEMALE THD","334 in","N/S","LEVER","Acid Water, Oil and Gas","5-100 deg"]
["0063385","SEAT: TYPE: DISC SAFETY VALVE; DIMENSIONS: SQ 0.514 IN; MATERIAL: 1.4122 DIN X 35CRMO17; SUPPL P/N: 018109610; 601267620; MODEL NO: VSE2.40.25.A.50.I.22.123; USED ON SEMPELL; POSITION CODE RL01S010, RL02S009, RL03S008","Sempell","DISC SAFETY VALVE","13.06MM","1.4122 DIN X 35CRMO17","N/A","1.4122 stainless steel seat with hardened/stainless disc interface","TBC","N/S","N/S","TBC","SEMPELL","up to 450"]
["0063532","VALVE, GATE: VALVE SIZE: 32 MM; TYPE: WEDGE; CONNECTION: THD; BODY MATERIAL: BRASS; TRIM: DISC/STEM BRS; OPERATED: HANDWHEEL; STEM DESIGN: NON RISING; STYLE: THD BONNET; TEMPERATURE RATING: 175 DEG C; DESIGN RATING: 1600 KPA; REFERENCE NO: 1001-125; SUPPLIER NOTE: TO BE SUPPLIED ACCORDING TO S.A.B.S. SPECIFICATION WITH A PRESSURE CERTIFICATE; CLASS 125","Pegler Yorkshire","GATE; WEDGE","32 MM","BRASS","1600 KPA","DISC/STEM BRS; NON RISING","THD","N/S","N/S","HANDWHEEL","AIR,WATER,OIL","175 DEG C"]
["0065784","VALVE: TYPE: MAIN CONTROL; VALVE SIZE: 100 MM; OPERATED: PRESSURE; BODY MATERIAL: STL; STYLE: 2 WAY; TRIM: BONNET STL; REFERENCE NO: MB9-642.6300C; CONNECTION MANIFOLD","Burckhardt Compression","MAIN CONTROL","100 MM","STL","N/A","BONNET STL","Manifold mounted","N/S","N/S","PRESSURE","Main Control","N/S"]
["0065929","VALVE, RELIEF: VALVE SIZE: 25 MM; SET PRESSURE: 1015 LB; CONNECTION: FNPT; BODY MATERIAL: CI; TRIM: DISC SS; SPRING STL; OPERATED: PRESSURE, SPRING; REFERENCE NO: 83C88-81; SAFETY; SERIES 80 SRV","Consolidated / Baker Hughes","RELIEF","25 MM","CI","1015 LB","DISC SS","FNPT","N/S","N/S","PRESSURE, SPRING","Safety / Pressure Relief","180 deg"]
["0066050","VALVE, GATE: VALVE SIZE: 1-1/2 IN; TYPE: SOLID WEDGE; CONNECTION: FNPT; BODY MATERIAL: BRASS; TRIM: DISC BRS; OPERATED: HANDWHEEL; STEM DESIGN: INSIDE SCREW; STYLE: THD BONNET; DESIGN RATING: 2000 KPA; COBRA","Cobra Watertech","GATE; SOLID WEDGE","1-1/2 IN","BRASS","2000 KPA","DISC BRS; INSIDE SCREW","FNPT","N/S","N/S","HANDWHEEL","water, hot water, and general fluid","5-80 deg"]
["0065807","VALVE: TYPE: FLOW CONTROL; VALVE SIZE: 15 MM; CONNECTION: FNPT; OPERATED: PRESSURE; BODY MATERIAL: STL; STYLE: 2 WAY; TRIM: BONNET STL; REFERENCE NO: PCM-600; FOR HIGH PRESSURE OIL FLOW; COLORFLOW","Colorflow","FLOW CONTROL","15 MM","STL","N/A","BONNET STL","FNPT","5Wvalve size: 15 mm; connection: fnpt; operated: pressure; body material: stl","N/S","PRESSURE","Flow Control (High Pressure Oil Flow)","−29 to +425 deg"]
["0065808","VALVE, GLOBE: VALVE SIZE: 3/4 IN; OPERATED: HANDWHEEL; CONNECTION: FLANGE; BODY MATERIAL: STL; TRIM: BONNET STL; STEM DESIGN: INSIDE SCREW; STYLE: BOLTED BONNET; REFERENCE NO: Y237A-4","Yarway","GLOBE","3/4 IN","STL","N/S","BONNET STL; INSIDE SCREW","FLANGE","5S/4 in","N/S","HANDWHEEL","liquid, steam, gas","40 to 120 deg"]
["0066072","VALVE, CHECK: TYPE: PISTON; VALVE SIZE: 25 MM; CONNECTION: NPT; BODY MATERIAL: STAINLESS STEEL; STYLE: THD CAP; TRIM: DISC/CAP STL; NON-RETURN; EO; TUBE SIZE 25MM OD EO TUBE CONNECTION AT BOTH ENDS","Parker Hannifin","CHECK; PISTON","25 MM","STAINLESS STEEL","N/S","DISC/CAP STL","NPT","190 mm","N/S","Hydraulic/tube system service","oil, hydraulic fluid, gas","−196 to +538 deg"]
["0065832","VALVE: TYPE: ISOLATING; VALVE SIZE: 65 MM; CONNECTION: THD; OPERATED: HANDWHEEL; BODY MATERIAL: STL; STYLE: THD BONNET; TRIM: DISC/STEM SS; PRESS TANK PUMP UNLOADER","Burckhardt Compression/Parker Hannifin/KSB","ISOLATING","65 MM","STL","N/S","DISC/STEM SS","THD","5Ove size: 65 mm; connection: thd","N/S","HANDWHEEL","pressure tank and pump unloader isolation","−29 to +425 deg"]
["0065847","VALVE, NEEDLE: VALVE SIZE: 60 MM; BODY MATERIAL: STL; FACE TO FACE LENGTH: 120 MM; REFERENCE NO: MB9-642-5362E; NOZZLE","Burckhardt Compression","NEEDLE","60 MM","STL","N/S","SS needle & stem with hardened nozzle seat and graphite packing","Nozzle connection","120 mm ","N/S","Flow regulation","precise flow control, throttling","up to 425 deg"]
["0065861","VALVE, PILOT: VALVE SIZE: 5 MM; MATERIAL: BRASS; REFERENCE NO: MB8-288-1705D; SIZE 6MM LG; CONNECTION COMPRESSION; STYLE 4 WAY; TRIM SS STEM; PRESSURE OPERATED; COMPLETE WITH PISTON; X5CRNI 189; GROUP 1700; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Burckhardt Compression","PILOT","5 MM","BRASS","N/S","SS piston & stem with brass seat and NBR/PTFE seals","COMPRESSION","95 mm","N/S","PRESSURE","Pilot / Control Service","up to 200 deg"]
["0066073","VALVE, RELIEF: VALVE SIZE: 12 MM; SET PRESSURE: 400 BAR; CONNECTION: FNPT; BODY MATERIAL: STL; TRIM: SPRING STL; OPERATED: PRESSURE, SPRING; REXROTH PRESSURE; HYDRONORMA","Rexroth","RELIEF","12 MM","STL","400 BAR","SPRING STL","FNPT","95 mm","N/S","PRESSURE, SPRING","AIR,WATER,OIL","−29 to +425 deg"]
["0065917","VALVE, RELIEF: VALVE SIZE: 45 X 40 MM; SET PRESSURE: 70 BAR; CONNECTION: NPT X FNPT; BODY MATERIAL: STL; TRIM: DISC/SPRING STL; OPERATED: PRESSURE, SPRING; SAFETY","Bopp & Reuther","RELIEF","45 X 40 MM","STL","70 BAR","DISC/SPRING STL","NPT X FNPT","N/S","N/S","PRESSURE, SPRING","AIR,WATER,OIL","up to 425 deg"]
["0066074","VALVE, BALL: VALVE SIZE: 16 MM; DESIGN RATING: 100 BAR; TEMPERATURE RATING: -200 TO 200 DEG C; CONNECTION: NPT X FNPT; BODY MATERIAL: STEEL; OPERATED: LEVER; STYLE: 4 WAY; TRIM: BALL STL; SPECIFICATION: DIN 3230; PORT TYPE: 3 X MALE; 1 X FEMALE; APPLICATION: UPSTREAM SEAL CHANGE OVER VALVE; TYPE: MANUAL OPERATED; SUPPL P/N: 1017489; REFERENCE NO: 1017489; 3 MALE X 1 FEMALE; CHANGE-OVER; BLOCK; ARGUS","Argus","BALL; 3 X MALE; MANUAL OPERATED","16 MM","STEEL","100 BAR","BALL STL","NPT X FNPT","95 mm","N/S","LEVER","UPSTREAM SEAL CHANGE OVER VALVE","-200 TO 200 DEG C"]
["0066234","VALVE, DIAPHRAGM: VALVE SIZE: 32 MM; CONNECTION: FNPT; BODY MATERIAL: CI; DIAPHRAGM MATERIAL: RUBBER GR Q; OPERATED: HANDWHEEL; STYLE: WEIR; SAUNDERS; TYPE A","Saunders","DIAPHRAGM","32 MM","CI; RUBBER GR Q","N/S","RUBBER GR Q","FNPT","A6 fnpt","N/S","HANDWHEEL","Isolation / throttling of corrosive, abrasive, slurry, water, chemical, and process fluids","up to 90 deg"]
["0066076","VALVE, NEEDLE: VALVE SIZE: 3.5 MM; CONNECTION: THD MALE X FEMALE; BODY MATERIAL: BRASS; OPERATED: HANDWHEEL; TRIM: DISC STL; THD BONNET; BLOCKING VALVE; P.17","Parker Hannifin","NEEDLE","3.5 MM","BRASS","N/S","DISC STL","THD MALE X FEMALE","6:3.5 mm","N/S","HANDWHEEL","AIR/OIL/WATER;","up to 200 deg"]
["0066235","VALVE, DIAPHRAGM: VALVE SIZE: 40 MM; CONNECTION: FNPT; BODY MATERIAL: CI; DIAPHRAGM MATERIAL: RUBBER GR Q; OPERATED: HANDWHEEL; STYLE: WEIR; SAUNDERS; TYPE A","Saunders","DIAPHRAGM","40 MM","CI; RUBBER GR Q","N/S","RUBBER GR Q","FNPT","A6 fnpt","N/S","HANDWHEEL","Sewage and wastewater, Water,Process water","up to 90 deg"]
["0066236","VALVE, DIAPHRAGM: VALVE SIZE: 50 MM; CONNECTION: FNPT; BODY MATERIAL: CI; DIAPHRAGM MATERIAL: RUBBER GR Q; OPERATED: HANDWHEEL; STYLE: WEIR; SAUNDERS","Saunders","DIAPHRAGM","50 MM","CI; RUBBER GR Q","N/S","RUBBER GR Q","FNPT","A6 fnpt","N/S","HANDWHEEL","Sewage and wastewater, Water,Process water","up to 90 deg"]
["0066205","VALVE, RELIEF: SET PRESSURE: 60 BAR; REFERENCE NO: MB8-222-2450C60B; SAFETY","Burckhardt Compression","RELIEF","N/S","STEEL","60 BAR","SS disc & seat, SS spindle, chrome alloy spring (metal-seated safety valve)","TBC","N/S","N/S","PRESSURE","Safety Protection","180 deg"]
["0066327","VALVE: TYPE: COMPENSATION; VALVE SIZE: 16 MM; CONNECTION: SLIP ON; OPERATED: LEVER; BODY MATERIAL: STAINLESS STEEL; STYLE: 3 WAY; TRIM: BONNET SS; GPS","GPS Valve (probable)","COMPENSATION","16 MM","STAINLESS STEEL","N/S","BONNET SS","SLIP ON","6Lvalve size: 16 mm; connection: slip on","N/S","LEVER","Air,Gas,Liquid","−196 to +538 deg"]
["0066223","VALVE, SOLENOID: PIPE SIZE: 25 MM; STYLE: 4 WAY; POTENTIAL: 110/120 VAC; DESIGN RATING: 3000 LB; BODY MATERIAL: STEEL; MEDIUM: OIL; CURRENT: 0.72-0.75 A; MODEL NO: D63W1B1Y 34; 50/60 HZ; CONNECTION MANIFOLD; GENERAL PURPOSE ENCLOSURE; DIRECTIONAL CONTROL VALVE","Yuken Kogyo","SOLENOID","25 MM","STEEL","3000 LB","Hardened steel spool with SS armature and NBR/PTFE seals","Manifold mounted","190 mm","N/S","SOLENOID","OIL","−29 to +425 deg"]
["0066232","VALVE, DIAPHRAGM: VALVE SIZE: 15 MM; CONNECTION: FNPT; BODY MATERIAL: CI; DIAPHRAGM MATERIAL: RUBBER GR Q; OPERATED: HANDWHEEL; STYLE: WEIR; REFERENCE NO: A; SAUNDERS","Saunders","DIAPHRAGM","15 MM","CI; RUBBER GR Q","N/S","RUBBER GR Q","FNPT","A6 fnpt","N/S","HANDWHEEL","Water, slurry, or compatible process fluid","20-90 deg"]
["0066233","VALVE, DIAPHRAGM: VALVE SIZE: 25 MM; CONNECTION: FNPT; BODY MATERIAL: CI; DIAPHRAGM MATERIAL: RUBBER GR Q; OPERATED: HANDWHEEL; STYLE: WEIR; SAUNDERS; TYPE A","Saunders","DIAPHRAGM","25 MM","CI; RUBBER GR Q","N/S","RUBBER GR Q","FNPT","A6 fnpt","N/S","HANDWHEEL","Water / Slurry Service","20-90 deg"]
["0066493","VALVE, CHECK: TYPE: PISTON; VALVE SIZE: 12 MM; CONNECTION: NPT; BODY MATERIAL: STL; STYLE: THD CAP; TRIM: DISC STL; SUPPL P/N: RHD12-PL; NON-RETURN; EO; TUBE CONNECTION AT BOTH ENDS","Parker Hannifin","CHECK; PISTON","12 MM","STL","N/S","DISC STL","NPT","190 mm","N/S","PRESSURE","Hydraulic oil/Low-flammability hydraulic fluids","20-120 deg"]
["0066494","SPOOL: TYPE: RELIEF VALVE; INSIDE DIAMETER: 108 MM; LENGTH: 153 MM; MATERIAL: STL; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Burckhardt Compression","RELIEF VALVE","108 MM","STL","N/S","Hardened steel spool with PTFE guide rings and hardened sealing surfaces","TBC","95 mm","N/S","PRESSURE","hydraulic oil / hydraulic fluid service","up to 425 deg"]
["0066522","VALVE, GATE: VALVE SIZE: 400 MM; TYPE: SOLID WEDGE; CONNECTION: FLANGE; BODY MATERIAL: STL; TRIM: BONNET STL; OPERATED: HANDWHEEL; STEM DESIGN: RISING OUTSIDE SCREW; STYLE: BOLTED BONNET; CAST; HYDRO TEST CERTIFICATE REQUIRED","Flowserve","GATE; SOLID WEDGE","400 MM","STL","ANSI Class 150/300/600","BONNET STL; RISING OUTSIDE SCREW","FLANGE","6R0 mm","N/S","HANDWHEEL","Industrial process fluid service","up to 425 deg"]
["0066523","VALVE, GATE: VALVE SIZE: 300 MM; TYPE: SOLID WEDGE; CONNECTION: FLANGE; BODY MATERIAL: STL CAST; TRIM: BONNET STL; OPERATED: HANDWHEEL, GEAR; STEM DESIGN: RISING OS; STYLE: BOLTED BONNET; DESIGN RATING: 100 BAR; HYDRO TEST CERTIFICATE REQUIRED; REFER TO CONTRACT OPY 49218","Velan","GATE; SOLID WEDGE","300 MM","STL CAST","100 BAR","BONNET STL; RISING OS","FLANGE","610 rilling / PCD, Mediumrilling / PCD, Medium","N/S","HANDWHEEL, GEAR","High-pressure industrial process service","up to 425 deg"]
["0066524","VALVE, GATE: VALVE SIZE: 250 MM; TYPE: SOLID WEDGE; CONNECTION: FLANGE; BODY MATERIAL: CS; TRIM: BONNET STL; OPERATED: HANDWHEEL; STEM DESIGN: RISING OUTSIDE SCREW; STYLE: BOLTED BONNET","Flowserve","GATE; SOLID WEDGE","250 MM","CS","ANSI Class 150/300/600","BONNET STL; RISING OUTSIDE SCREW","FLANGE","6A0 mm","N/S","HANDWHEEL","High-pressure industrial process service","150 deg"]
["0066525","VALVE, GATE: VALVE SIZE: 200 MM; CONNECTION: FLANGE; BODY MATERIAL: STL CAST; TRIM: BONNET STL; OPERATED: HANDWHEEL; STEM DESIGN: RISING OS; STYLE: BOLTED BONNET","Flowserve","GATE","200 MM","STL CAST","ANSI Class 150/300/600","BONNET STL; RISING OS","FLANGE","6E0 mm","N/S","HANDWHEEL","High-pressure industrial process service","150 deg"]
["0066530","VALVE: VALVE SIZE: 250 MM; BODY MATERIAL: CS; FIG NO: 16SMZ; NON-RETURN; SIZE 10; HYDRO.TEST CERTIFICATE REQUIRED FOR ALL VALVES","Check-Rite Valves","Non-return valve / Check valve","250 MM","CS","N/S","SS disc, hard-faced seat, SS hinge, graphite/PTFE seals","TBC","E6 cs","N/S","PRESSURE","Process fluid service","150 deg"]
["0066527","VALVE, BUTTERFLY: TYPE: WAFER; VALVE SIZE: 400 MM; CONNECTION: FLANGE; BODY MATERIAL: CS; OPERATED: GEAR; TRIM: DISC STL RUBBERIZED; REFERENCE NO: 051100A492183; BOVING; COMPLETE WITH MASTERGEAR OPERATOR AND HANDWHEEL; HYDRO TEST CERTIFICATE REQUIRED FOR ALL VALVES","Boving","BUTTERFLY; WAFER","400 MM","CS","N/S","DISC STL RUBBERIZED","FLANGE","95 mm","N/S","GEAR","Industrial process fluid service","80 deg"]
["0066531","VALVE, CHECK: TYPE: SWING; VALVE SIZE: 80 MM; CONNECTION: COMPRESSION; BODY MATERIAL: CS; TRIM: DISC STL; FIG NO: 16SMZ; CHECKRITE NON-RETURN; HYDRO TEST CERTIFICATE REQUIRED FOR ALL VALVES","Check-Rite Valves","CHECK; SWING","80 MM","CS","N/S","DISC STL","COMPRESSION","190 mm","N/S","PRESSURE","Process fluid service","150 deg"]
["0066529","VALVE, CHECK: TYPE: SWING; VALVE SIZE: 400 MM; DESIGN RATING: 16 BAR; CONNECTION: FLANGE; BODY MATERIAL: CS; TRIM: BONNET/DISC STEEL; REFERENCE NO: 16SMZ; CHECKRITE NON-RETURN; HYDRO. TEST CERTIFICATE REQUIRED FOR ALL VALVES","Check-Rite Valves","CHECK; SWING","400 MM","CS","16 BAR","BONNET/DISC STEEL","FLANGE","6:valve size: 400 mm; design rating: 16 bar; connection: flange","N/S","PRESSURE","Process fluid service","150 deg"]
["0069572","VALVE, GATE: VALVE SIZE: 40 MM; CONNECTION: FLANGE; OPERATED: HANDWHEEL; FIG NO: H9-107; REFERENCE NO: W.P.9/1500; BONNEY FORGE","Bonney Forge","GATE","40 MM","STEAT","1500 PSI (WP) / Class 1500 Equivalent","(410 SS + Stellite hardfacing) for industrial pipeline gate valves","FLANGE","N/S","N/S","HANDWHEEL","Industrial/process service","250 deg"]
["0066533","VALVE, RELIEF: VALVE SIZE: 200 MM; BODY MATERIAL: STL CAST; OPERATED: PRESSURE; CAT NO: 50A-01B; CLAYTON","Cla-Val (Clayton)","RELIEF","200 MM","STL CAST","N/S","N/S","TBC","95 mm","N/S","PRESSURE","Pressure relief service for process systems","80 deg"]
["0066534","VALVE: TYPE: DELUGE; VALVE SIZE: 150 MM; DESIGN RATING: 150 LB; CONNECTION: FLANGE; OPERATED: AIR; BODY MATERIAL: BRASS; STYLE: 2 WAY; TRIM: BONNET BRS; SPECIFICATION: BS 4504; N.P. 16/3","Claval","DELUGE","150 MM","BRASS","150 LB","BONNET BRS","FLANGE","N/S","N/S","AIR","Fire protection / water deluge system service","50 deg"]
["0066535","VALVE, BALL: VALVE SIZE: 1/2 IN; DESIGN RATING: 40 LB; TEMPERATURE RATING: 25 DEG C; CONNECTION: FNPT; BODY MATERIAL: STAINLESS STEEL; OPERATED: LEVER; STYLE: UNION BONNET; TRIM: BALL SS; BRASS; WITH FIXED FEMALE FLANGE EITHER END","Swagelok","BALL","1/2 IN","STAINLESS STEEL","40 LB","BALL SS","FNPT","N/S","N/S","LEVER","General process/instrument service","25 DEG C"]
["0066661","VALVE, RELIEF: VALVE SIZE: 20 MM; BODY MATERIAL: STL; TRIM: BONNET/SPRING STL; OPERATED: PRESSURE; REFERENCE NO: 936-36275; L.P.; ABEX DENISON; MANIFOLD","Denison Hydraulics (formerly Abex-Denison)","RELIEF","20 MM","STL","N/S","BONNET/SPRING STL","TBC","N/S","N/S","PRESSURE","Hydraulic pressure relief service","80 deg"]
["0067279","VALVE, BUTTERFLY: TYPE: WAFER; VALVE SIZE: 65 MM; DESIGN RATING: 16 BAR; CONNECTION: CLAMP; BODY MATERIAL: CI; OPERATED: LEVER; TRIM: DISC/SHAFT SS GR 316; SEAT EPDM; REFERENCE NO: 065-515-6S; DISC/SHAFT HEXAGON MACHINED CENTRE HOLE; LINER: E.P.D.M; SEAT TEST PRESSURE: 18 BAR; BODY TEST PRESSURE: 24 BAR; MATERIAL AND TEST CERTIFICATES TO DIN 50049/3.1B ARE TO BE SUPPLIED ON DELIVERY","Boehmer (probable)","BUTTERFLY; WAFER","65 MM","CI","16 BAR","DISC/SHAFT SS GR 316","CLAMP","95 mm","N/S","LEVER","Water/process fluid service","80 deg"]
["0068148","VALVE, RELIEF: VALVE SIZE: 50 MM; SET PRESSURE: 35 KPA; CONNECTION: THD; BODY MATERIAL: STL; TRIM: BRASS; OPERATED: SPRING; PRESSURE RANGE: 2-20 LB; REFERENCE NO: MD0014; SAFETY; TYPE 616-2; TYPE: HLP","Hale Hamilton","RELIEF; HLP","50 MM","STL","2-20 LB; 35 KPA","BRASS","THD","100 mm","N/S","SPRING","Pressure relief service","80 deg"]
["0068767","VALVE: TYPE: CONTROL; VALVE SIZE: 12 MM; CONNECTION: FNPT; OPERATED: PRESSURE; BODY MATERIAL: STL; STYLE: 4 WAY; TRIM: DISC STL; REFERENCE NO: MB9-642-6500B; SIZE 15MM THK; FOR LOCKING VALVE 620/1","Burckhardt Compression","CONTROL","12 MM","STL","N/S","DISC STL","FNPT","N/S","N/S","PRESSURE","Control/locking valve service","80 deg"]
["0068909","ASSEMBLY: TYPE: BFPT DISCHARGE ISOLATOR VALVE BELT; SUPPL P/N: 324-39; FIG NO: M279400W; BRISCH CODE: L9571-501 HOPKINSONS VALVE, 100NB","Hopkinsons Valve","100NB; BFPT DISCHARGE ISOLATOR VALVE BELT","100 MM","Not specified","N/S","N/S","TBC","N/S","N/S","TBC","water system application","TBC"]
["0068910","VALVE, GLOBE: VALVE SIZE: 1/2 IN; OPERATED: HANDWHEEL; CONNECTION: BW; BODY MATERIAL: CS ASTM A105; TRIM: DISC/SEAT HF; STEM SS GR 410; STEM DESIGN: RISING SPINDLE; STYLE: INTEGRAL BONNET; Y BODY; DESIGN RATING: 2500 PSI; TEMPERATURE RATING: 840 DEG F; REFERENCE NO: 578; VELAN","Velan","GLOBE","1/2 IN","CS ASTM A105","2500 PSI","DISC/SEAT HF; RISING SPINDLE","BW","N/S","N/S","HANDWHEEL","High-pressure process service","840 DEG F"]
["0072009","VALVE, BALL: VALVE SIZE: 16 MM; DESIGN RATING: 400 LB; CONNECTION: FNPT; BODY MATERIAL: STEEL; OPERATED: LEVER; STYLE: 2 WAY; TRIM: BALL STL; SUPPL P/N: BH-B400-716; BOHMER; BLOCK","Bohmer","BALL","16 MM","STEEL","400 LB","BALL STL","FNPT","N/S","N/S","LEVER","High-pressure process fluid service","150 deg"]
["0070478","VALVE, RELIEF: VALVE SIZE: 50 X 32 MM; SET PRESSURE: 600 KPA; TEMPERATURE RATING: -10 TO 14 DEG C; CONNECTION: FLANGE; BODY MATERIAL: CI; TRIM: STAINLESS STEEL; OPERATED: PRESSURE; DESIGN RATING: 16 BAR; PRESSURE RANGE: 6 BAR; FIG NO: 4411/H2; REFERENCE NO: 16; SAFETY; INLET AND OUTLET PN16; TO SIZED TO DIN3320 AND TEST APPROVED IN ACCORDANCE WITH (AD-MERKBLATT A2); FLOW CAPACITY TO BE AT LEAST 35000 KG/HR","HEROSE","RELIEF","50 X 32 MM","CI","16 BAR; 6 BAR; 600 KPA","STAINLESS STEEL","FLANGE","95 mm","N/S","PRESSURE","Pressure relief service","-10 TO 14 DEG C"]
["0072010","VALVE, BALL: VALVE SIZE: 20 MM; DESIGN RATING: 315; CONNECTION: FNPT; BODY MATERIAL: STEEL; OPERATED: LEVER; STYLE: 2 WAY; TRIM: BALL STL; BLOCK; BOHMER","Bohmer","BALL","20 MM","STEEL",315,"BALL STL","FNPT","95 mm","N/S","LEVER","Process fluid / hydraulic service","150 deg"]
["0072012","VALVE, BALL: VALVE SIZE: 50 MM; DESIGN RATING: 6 BAR; CONNECTION: FLANGE; BODY MATERIAL: STEEL; OPERATED: LEVER; STYLE: 2 WAY; TRIM: BALL STL; BOHMER; SERIES FK","Bohmer","BALL","50 MM","STEEL","6 BAR","BALL STL","FLANGE","95 mm","N/S","LEVER","Process fluid service","150 deg"]
["0072002","VALVE, BALL: VALVE SIZE: 50 MM; DESIGN RATING: 100 BAR; CONNECTION: FLANGE; BODY MATERIAL: STEEL; OPERATED: LEVER; STYLE: 2 WAY; TRIM: BALL STL; BOHMER","Bohmer","BALL","50 MM","STEEL","100 BAR","BALL STL","FLANGE","95 mm","N/S","LEVER","High-pressure process fluid service","150 deg"]
["0072004","VALVE, BALL: VALVE SIZE: 40 MM; DESIGN RATING: 100; CONNECTION: FNPT; BODY MATERIAL: STEEL; OPERATED: LEVER; STYLE: 2 WAY; TRIM: BALL STL; GRADE: C22.8; REFERENCE NO: 3101-0040-598166; SHUT-OFF; ARGUS","Argus","BALL","40 MM","STEEL",100,"BALL STL","FNPT","N/S","N/S","LEVER","Shut-off/isolation service","150 deg"]
["0072013","VALVE, BALL: VALVE SIZE: 10 MM; DESIGN RATING: 500 LB; CONNECTION: FNPT; BODY MATERIAL: STEEL; OPERATED: LEVER; STYLE: 2 WAY; TRIM: BALL STL; SUPPL P/N: BH-B500-710; BOHMER; BLOCK","Bohmer","BALL","10 MM","STEEL","500 LB","BALL STL","FNPT","N/S","N/S","LEVER","High-pressure process fluid service","150 deg"]
["0072006","VALVE, BALL: VALVE SIZE: DN 65 MM; DESIGN RATING: PN100; CONNECTION: FLANGE; REFERENCE NO: 3121-0065-530401; SHUT OFF; COMPLETE WITH HANDLE 350 K","Bohmer","BALL","DN 65 MM","STEEL","PN100","N/S","FLANGE","N/S","N/S","HAND","Shut-off/isolation service","150 deg"]
["0072007","VALVE, BALL: VALVE SIZE: 16 MM; DESIGN RATING: 400 LB; CONNECTION: NPT; BODY MATERIAL: STEEL; OPERATED: LEVER; STYLE: 2 WAY; TRIM: BALL STL; BOHMER BLOCK","Bohmer","BALL","16 MM","STEEL","400 LB","BALL STL","NPT","95 mm","N/S","LEVER","Process fluid isolation/shut-off service","150 deg"]
["0072008","VALVE, BALL: VALVE SIZE: 10 MM; DESIGN RATING: 315; CONNECTION: NPT; BODY MATERIAL: STEEL; OPERATED: LEVER; STYLE: 4 WAY; TRIM: BALL STL; SUPPL P/N: VH-VX315-210; REFERENCE NO: VX315-210; BOHMER; BLOCK","Bohmer","BALL","10 MM","STEEL",315,"BALL STL","NPT","N/S","N/S","LEVER","Process fluid isolation/control service","80 deg"]
["0072014","VALVE, BALL: VALVE SIZE: 20 MM; DESIGN RATING: 315; CONNECTION: NPT; BODY MATERIAL: STEEL; OPERATED: LEVER; STYLE: 2 WAY; TRIM: BALL STL; BLOCK; BOHMER","Bohmer","BALL","20 MM","STEEL",315,"BALL STL","NPT","95 mm","N/S","LEVER","Process fluid isolation/shut-off service","80 deg"]
["0072026","VALVE, RELIEF: VALVE SIZE: 13 MM; SET PRESSURE: 240 LB; CONNECTION: NPT; BODY MATERIAL: BRASS; TRIM: DISC BRS; SPRING STL; OPERATED: PRESSURE, SPRING; SUPPL P/N: 98650/1172; SECOND STAGE SAFETY","Haskel Energy Systems (probable)","RELIEF","13 MM","BRASS","240 LB","DISC BRS","NPT","50 mm","N/S","PRESSURE, SPRING","Pressure relief service","80 deg"]
["0072016","VALVE, BALL: VALVE SIZE: 8 MM; DESIGN RATING: 500 LB; CONNECTION: FNPT; BODY MATERIAL: STEEL; OPERATED: LEVER; STYLE: 2 WAY; TRIM: BALL STL; BOHMER; BLOCK","Bohmer","BALL","8 MM","STEEL","500 LB","BALL STL","FNPT","95 mm","N/S","LEVER","Process fluid isolation/shut-off service","150 deg"]
["0072017","VALVE, BALL: VALVE SIZE: 6 MM; DESIGN RATING: 500 LB; CONNECTION: FNPT; BODY MATERIAL: STEEL; OPERATED: LEVER; STYLE: 2 WAY; TRIM: BALL STL; BOHMER; BLOCK","Bohmer","BALL","6 MM","STEEL","500 LB","BALL STL","FNPT","95 mm","N/S","LEVER","Process fluid isolation/shut-off service","150 deg"]
["0072018","VALVE, GLOBE: VALVE SIZE: 4 MM; OPERATED: HANDWHEEL; CONNECTION: NPT; BODY MATERIAL: STL A122; TRIM: SPINDLE 4122; STEM DESIGN: INSIDE SCREW; STYLE: THD BONNET; DESIGN RATING: 400 BAR; ERMETO HIGH PRESSURE; TUBE SIZE OD 8 MM","Parker Hannifin (Ermeto)","GLOBE","4 MM","STL A122","400 BAR","SPINDLE 4122; INSIDE SCREW","NPT","P2 handwheel","N/S","HANDWHEEL","High-pressure instrumentation / hydraulic service","150 deg"]
["0072020","VALVE, CHECK: TYPE: PISTON; VALVE SIZE: 12 MM; CONNECTION: FNPT; BODY MATERIAL: STL; STYLE: THD CAP; TRIM: DISC STL; BRAKE AIR COMPRESS","Parker Hannifin (probable)","CHECK; PISTON","12 MM","STL","N/S","DISC STL","FNPT","190 mm","N/S","PRESSURE","Brake air compressor service","150 deg"]
["0072021","VALVE, RELIEF: VALVE SIZE: 12 MM; CONNECTION: NPT; BODY MATERIAL: STL; TRIM: SPRING STL; OPERATED: PRESSURE, SPRING; REFERENCE NO: 98650-1162; OIL REGULATOR","Haskel Energy Systems","RELIEF","12 MM","STL","N/S","SPRING STL","NPT","2N12 mm","N/S","PRESSURE, SPRING","Oil regulator service","80 deg"]
["0072022","VALVE, RELIEF: VALVE SIZE: 12 MM; SET PRESSURE: 42 LB; CONNECTION: NPT; BODY MATERIAL: BRASS; TRIM: DISC BRS; SPRING STL; OPERATED: PRESSURE, SPRING; SUPPL P/N: 98650/1171; FIRST STAGE SAFETY; SEETRU; 311100200 C1940","Seetru Limited","RELIEF","12 MM","BRASS","42 LB","DISC BRS","NPT","5; mm","N/S","PRESSURE, SPRING","Safety pressure relief service","80 deg"]
["0072023","VALVE: TYPE: DISCHARGE; VALVE SIZE: 51 MM; OPERATED: PRESSURE; BODY MATERIAL: STL; TRIM: DISC STL; SUPPL P/N: 98650/1180; CONNECTION COMPRESSION; FIRST STAGE DELIVERY","Haskel Energy Systems","DISCHARGE","51 MM","STL","N/S","DISC STL","COMPRESSION","4D: PRESSURE; e-to-Face, Drilling / PCD, Mediume-to-Face, Drilling / PCD, Medium","N/S","PRESSURE","First stage delivery/discharge service","120 deg"]
["0072024","VALVE: TYPE: COMPRESSOR; VALVE SIZE: 8 MM; CONNECTION: THD FEMALE; OPERATED: PRESSURE; BODY MATERIAL: STL; STYLE: 6 WAY; TRIM: BONNET/DISC STL; REFERENCE NO: 98650-1161; 4TH STAGE; SIZE 11MM THK","Haskel Energy Systems","COMPRESSOR","8 MM","STL","N/S","BONNET/DISC STL","THD FEMALE","2 lve size: 8 mm; connection: thd female; operated: pressure; body material: stl","N/S","PRESSURE","Compressor stage service","180 deg"]
["0072027","VALVE, RELIEF: VALVE SIZE: 13 MM; SET PRESSURE: 1160 LB; CONNECTION: NPT; BODY MATERIAL: BRASS; TRIM: DISC BRS; SPRING STL; OPERATED: PRESSURE, SPRING; SUPPL P/N: 98650/1173; THIRD STAGE SAFETY; SEETRU","Seetru Limited","RELIEF","13 MM","BRASS","1160 LB","DISC BRS","NPT","560 mm","N/S","PRESSURE, SPRING","High-pressure safety relief service","150 deg"]
["0072029","VALVE: TYPE: DISCHARGE; VALVE SIZE: 34 MM; CONNECTION: COMPRESSION; OPERATED: PRESSURE; BODY MATERIAL: MS; TRIM: DISC STL; SUPPL P/N: 98650/1182; SECOND STAGE DELIVERY","Haskel Energy Systems","DISCHARGE","34 MM","Not specified","N/S","DISC STL","COMPRESSION","2Dve size: 34 mm; connection: compression","N/S","PRESSURE","Second stage delivery/discharge service","140 deg"]
["0072030","HOUSING: TYPE: VALVE; DIMENSIONS: DIA 34 X LG 62 MM; MATERIAL: ALUMINIUM; REFERENCE NO: C200604; SECOND STAGE, COVER; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Haskel Energy Systems","VALVE","3.5 MM","ALUMINIUM","N/S","N/S","TBC","N/S","N/S","TBC","Second stage valve assembly component","150 deg"]
["0072031","VALVE: TYPE: COMPRESSOR; VALVE SIZE: 9 MM; CONNECTION: THD FEMALE; OPERATED: PRESSURE; STYLE: 4 WAY; TRIM: DISC STL; SUPPL P/N: 98650/1160; THIRD STAGE VALVE; SIZE 12MM LG X 14MM THK","Haskel Energy Systems","COMPRESSOR","9 MM","STEYP","N/S","DISC STL","THD FEMALE","4ION: THD -to-Face, Drilling / PCD, Medium-to-Face, Drilling / PCD, Medium","N/S","PRESSURE","Compressor stage service","180 deg"]
["0072032","VALVE, RELIEF: VALVE SIZE: 13 MM; SET PRESSURE: 138 BAR; CONNECTION: NPT; BODY MATERIAL: STAINLESS STEEL; TRIM: BONNET SS; SPRING STL; OPERATED: PRESSURE; SUPPL P/N: 98661/1011","Haskel Energy Systems","RELIEF","13 MM","STAINLESS STEEL","138 BAR","BONNET SS","NPT","58 mm","N/S","PRESSURE","High-pressure pressure relief service","80 deg"]
["0072033","VALVE, RELIEF: VALVE SIZE: 12 MM; CONNECTION: NPT; BODY MATERIAL: STAINLESS STEEL; TRIM: SPRING STL; OPERATED: PRESSURE, SPRING; SUPPL P/N: 98261/1594/1525; SAFETY; OLD S P/N 98661/1010","Haskel Energy Systems","RELIEF","12 MM","STAINLESS STEEL","N/S","SPRING STL","NPT","2E12 mm","N/S","PRESSURE, SPRING","Safety pressure relief service","80 deg"]
["0072034","VALVE, RELIEF: VALVE SIZE: 34 MM; CONNECTION: FLANGE; BODY MATERIAL: CI; TRIM: SPRING STL; OPERATED: PRESSURE, SPRING; ITEM 20","HEROSE (probable)","RELIEF","34 MM","CI","N/S","SPRING STL","FLANGE","2R34 mm","N/S","PRESSURE, SPRING","Pressure relief service","80 deg"]
["0072035","VALVE, RELIEF: REFERENCE NO: L16; L-16; 503D","Haskel Energy Systems (probable)","RELIEF","N/S","STEEL","N/S","N/S","TBC","N/S","N/S","PRESSURE","Pressure relief servic","80 deg"]
["0072036","VALVE, CHECK: VALVE SIZE: 14 X 12 MM; CONNECTION: NPT; BODY MATERIAL: BRASS; STYLE: THD CAP; TRIM: CAP/SLEEVE BRS; SUPPL P/N: SCD-6504; 633; MODEL NO: 5H12; REFERENCE NO: PT633; 32001117; TYPE LIFT; WITH SLEEVE AND 12.7MM NUT; FOR INGERSOL FIRE PROTECTION COMPRESSOR","LIFT","CHECK","14 X 12 MM","BRASS","N/S","CAP/SLEEVE BRS","NPT","95 mm","N/S","PRESSURE","compressed air/gas service","80 deg"]
["0072037","VALVE: TYPE: BARE; VALVE SIZE: 48 MM; CONNECTION: FLANGE; OPERATED: PRESSURE; BODY MATERIAL: STAINLESS STEEL; TRIM: PLATE SS; REFERENCE NO: 1-32; 1095","Haskel Energy Systems (probable)","BARE","48 MM","STAINLESS STEEL","N/S","PLATE SS","FLANGE","2Mze: 48 mm; connection: flange","N/S","PRESSURE","Pressure operated valve service","150 deg"]
["0072038","VALVE, GLOBE: VALVE SIZE: 3 IN; OPERATED: HANDWHEEL; CONNECTION: FLANGE; BODY MATERIAL: CS; TRIM: DISC/SEAT 13CR; GRADE: WCB; STEM DESIGN: RISING OUTSIDE SCREW; STYLE: BOLTED BONNET; DESIGN RATING: 150 LB; REFERENCE NO: 2H18802; HIRATA","Hirata","GLOBE","3 IN","CS","150 LB","DISC/SEAT 13CR; RISING OUTSIDE SCREW","FLANGE","SCREW; STYLE: BOLTED BONNET; DESIGN RATING: 150 LB; REFERENCE NO: 2SCREW; STYLE: BOLTED BONNET; DESIGN RATING: 150 LB; REFERENCE NO: 2 mm","N/S","HANDWHEEL","Isolation/control service","200 deg"]
["0072039","VALVE, GLOBE: VALVE SIZE: 4 IN; OPERATED: HANDWHEEL; CONNECTION: FLANGE; BODY MATERIAL: CS; TRIM: SEAT 13CR; GRADE: WCB; STEM DESIGN: INSIDE SCREW; STYLE: BOLTED BONNET; DESIGN RATING: 150 LB; REFERENCE NO: 2H18629; HIRATA","Hirata","GLOBE","4 IN","CS","150 LB","SEAT 13CR; INSIDE SCREW","FLANGE","N/S","N/S","HANDWHEEL","Isolation/control service","200 deg"]
["0072040","VALVE, GATE: VALVE SIZE: 3 IN; TYPE: SOLID WEDGE; CONNECTION: FLANGE; BODY MATERIAL: STEEL; TRIM: SEAT 13CR; OPERATED: HANDWHEEL; STEM DESIGN: RISING OUTSIDE SCREW; STYLE: BOLTED BONNET; GRADE: WCB; DESIGN RATING: 150 LB; REFERENCE NO: 2H27347; CAST; HIRATA","Hirata","GATE; SOLID WEDGE","3 IN","STEEL","150 LB","SEAT 13CR; RISING OUTSIDE SCREW","FLANGE","210 mm","N/S","HANDWHEEL","Isolation service","200 deg"]
["0072041","VALVE, GLOBE: VALVE SIZE: 2 IN; OPERATED: HANDWHEEL; CONNECTION: FLANGE; BODY MATERIAL: CS; TRIM: DISC 13CR; GRADE: WCB; STEM DESIGN: RISING OUTSIDE SCREW; STYLE: BOLTED BONNET; DESIGN RATING: 600 LB; DRAWING NO: 2H18630 REV 1; HIRATA; SIZE 50 MM","Hirata","GLOBE","2 IN","CS","600 LB","DISC 13CR; RISING OUTSIDE SCREW","FLANGE","N/S","N/S","HANDWHEEL","Isolation/control service","250 deg"]
["0072042","VALVE, CHECK: VALVE SIZE: 2 IN; DESIGN RATING: 600 LB; CONNECTION: FLANGE; BODY MATERIAL: CS; DRAWING NO: 2H33514 REV 1; TYPE LIFT; HIRATA","LIFT; Hirata","CHECK","2 IN","CS","600 LB","Stainless steel 410 (AISI 410 SS) or 316 SS (depending on service)","FLANGE","N/S","N/S","PRESSURE","Flow control / backflow prevention service","250 deg"]
["0072043","VALVE, GLOBE: VALVE SIZE: 10 MM; OPERATED: HANDWHEEL; CONNECTION: FNPT; BODY MATERIAL: STL FORGED; TRIM: SEAT 13CR; STEM DESIGN: RISING OUTSIDE SCREW; STYLE: BOLTED BONNET; DESIGN RATING: 150-800 LB; DRAWING NO: 2N18553 REV 1; HIRATA","Hirata","GLOBE","10 MM","STL FORGED","150-800 LB","SEAT 13CR; RISING OUTSIDE SCREW","FNPT","1008 mm","N/S","HANDWHEEL","Isolation/control service","300 deg"]
["0072044","VALVE, GATE: VALVE SIZE: 1/2 IN; TYPE: WEDGE; CONNECTION: THD TAPER FEMALE; BODY MATERIAL: BRS CAST; TRIM: BRASS; OPERATED: HANDWHEEL; STEM DESIGN: NON RISING; STYLE: THD BONNET; SPECIFICATION: SABS 776; DESIGN RATING: 1600 KPA; TEMP RATING 880 KPA AT 175 DEG C; FULLWAY; CLASS 8; BONNET TYPE HEAD; GUIDED; WORKING PRESSURE 880 KPA AT 100 DEG C; HYDRAULIC WORKING PRESSURE 1600 KPA; TESTED TO 2000 KPA; BEARING THE SABS MARK OF APPROVAL","HEAD","GATE; WEDGE","1/2 IN","BRS CAST","1600 KPA","BRASS; NON RISING","THD TAPER FEMALE","N/S","N/S","HANDWHEEL","Isolation service","100 deg"]
["0072045","VALVE, GLOBE: VALVE SIZE: 4 IN; OPERATED: HANDWHEEL; CONNECTION: FLANGE; BODY MATERIAL: CS; TRIM: SEAT 13CR; GRADE: WCB; STEM DESIGN: RISING OUTSIDE SCREW; STYLE: BOLTED BONNET; DESIGN RATING: 150 LB; REFERENCE NO: 2H18803; 4820-70-5093043; HIRATA; SIZE: 100 MM","Hirata","GLOBE","4 IN","CS","150 LB","SEAT 13CR; RISING OUTSIDE SCREW","FLANGE","N/S","N/S","HANDWHEEL","Isolation/control service","200 deg"]
["0072046","VALVE, GATE: VALVE SIZE: 2-1/2 IN; CONNECTION: FLANGE; BODY MATERIAL: CS; DESIGN RATING: 150 LB; DRAWING NO: 2H27346 REV 1","Hopkinsons Valve (probable)","GATE","2-1/2 IN","CS","150 LB","N/S","FLANGE","190 mm","N/S","HANDWHEEL","Isolation service","200 deg"]
["0072047","VALVE, GATE: VALVE SIZE: 5 IN; CONNECTION: FLANGE; BODY MATERIAL: CS; TRIM: BONNET STL; OPERATED: HANDWHEEL; STEM DESIGN: RISING OUTSIDE SCREW; STYLE: BOLTED BONNET; DESIGN RATING: 150 LB; REFERENCE NO: 2H27348; HIRATA","Hirata","GATE","5 IN","CS","150 LB","BONNET STL; RISING OUTSIDE SCREW","FLANGE","N/S","N/S","HANDWHEEL","Isolation service","200 deg"]
["0072048","VALVE, GATE: VALVE SIZE: 150 MM; CONNECTION: FLANGE; BODY MATERIAL: CS; TRIM: SEAT 13CR; OPERATED: HANDWHEEL; STEM DESIGN: RISING OUTSIDE SCREW; STYLE: BOLTED BONNET; GRADE: WCB; DESIGN RATING: 150 LB; REFERENCE NO: 2H27349; HIRATA","Hirata","GATE","150 MM","CS","150 LB","SEAT 13CR; RISING OUTSIDE SCREW","FLANGE","N/S","N/S","HANDWHEEL","Isolation service","200 deg"]
["0072059","VALVE, GLOBE: VALVE SIZE: 1/2 IN; OPERATED: HANDWHEEL; CONNECTION: FNPT; BODY MATERIAL: STEEL; TRIM: DISC/SEAT SS GR 316; STEM DESIGN: INSIDE SCREW; STYLE: THD BONNET; DESIGN RATING: 150-200 LB; DRAWING NO: 2S18669 REV 1; HIRATA; MATERIAL SUSF316-97","Hirata","GLOBE","1/2 IN","STEEL","150-200 LB","DISC/SEAT SS GR 316; INSIDE SCREW","FNPT","N/S","N/S","HANDWHEEL","Isolation/control service","200 deg"]
["0072050","VALVE, ANGLE: TYPE: NEEDLE; VALVE SIZE: 200 MM; DESIGN RATING: 300 LB; CONNECTION: FLANGE; BODY MATERIAL: STL CAST; OPERATED: HANDWHEEL, GEAR; STYLE: BOLTED BONNET; TRIM: BONNET/DISC STL; GRADE: WCB 8B; DRAWING NO: HIRATA 2H18923 REV 1; REFERENCE NO: 2H18923","Hirata","ANGLE; NEEDLE","200 MM","STL CAST","300 LB","BONNET/DISC STL","FLANGE","95 mm","N/S","HANDWHEEL, GEAR","Flow regulation/isolation service","250 deg"]
["0072052","VALVE, GATE: VALVE SIZE: 50 MM; TYPE: SOLID WEDGE; CONNECTION: FLANGE; BODY MATERIAL: STEEL; TRIM: DISC 13CR; OPERATED: HANDWHEEL; STEM DESIGN: RISING OUTSIDE SCREW; STYLE: BOLTED BONNET; GRADE: WCB; DESIGN RATING: 600 LB; REFERENCE NO: 2H27350; CAST; HIRATA","Hirata","GATE; SOLID WEDGE","50 MM","STEEL","600 LB","DISC 13CR; RISING OUTSIDE SCREW","FLANGE","260 mm","N/S","HANDWHEEL","Isolation service","300 deg"]
["0072053","VALVE, GATE: VALVE SIZE: 3 IN; TYPE: SOLID WEDGE; CONNECTION: FLANGE; BODY MATERIAL: STEEL; TRIM: SEAT 13CR; OPERATED: HANDWHEEL; STEM DESIGN: RISING OUTSIDE SCREW; STYLE: BOLTED BONNET; GRADE: WCB; DESIGN RATING: 600 LB; REFERENCE NO: 2H27351; CAST; HIRATA","Hirata","GATE; SOLID WEDGE","3 IN","STEEL","600 LB","SEAT 13CR; RISING OUTSIDE SCREW","FLANGE","260 mm","N/S","HANDWHEEL","Isolation service","300 deg"]
["0072054","VALVE, GLOBE: VALVE SIZE: 100 MM; OPERATED: HANDWHEEL; CONNECTION: FLANGE; BODY MATERIAL: CS; TRIM: SEAT 13CR; GRADE: WCB; STEM DESIGN: RISING OUTSIDE SCREW; STYLE: BOLTED BONNET; DESIGN RATING: 600 LB; REFERENCE NO: 2H18626; HIRATA","Hirata","GLOBE","100 MM","CS","600 LB","SEAT 13CR; RISING OUTSIDE SCREW","FLANGE","N/S","N/S","HANDWHEEL","Isolation/control service","300 deg"]
["0072055","VALVE, CHECK: TYPE: SWING; VALVE SIZE: 100 MM; DESIGN RATING: 600 LB; CONNECTION: FLANGE; BODY MATERIAL: CS; STYLE: BOLTED CAP; TRIM: BONNET STL; REFERENCE NO: 2H33536; HIRATA","Hirata","CHECK; SWING","100 MM","CS","600 LB","BONNET STL","FLANGE","N/S","N/S","PRESSURE","Backflow prevention service","300 deg"]
["0072056","VALVE, GATE: VALVE SIZE: 1/2 IN; TYPE: SOLID WEDGE; CONNECTION: FLANGE; BODY MATERIAL: STEEL; TRIM: SEAT 13CR; OPERATED: HANDWHEEL; STEM DESIGN: INSIDE SCREW; STYLE: BOLTED BONNET; DESIGN RATING: 150-800 LB; REFERENCE NO: 2M27352; FORGED; HIRATA","Hirata","GATE; SOLID WEDGE","1/2 IN","STEEL","150-800 LB","SEAT 13CR; INSIDE SCREW","FLANGE","210-800 mm","N/S","HANDWHEEL","Isolation service","350 deg"]
["0072057","VALVE, GATE: VALVE SIZE: 100 MM; CONNECTION: FLANGE; BODY MATERIAL: CS; DESIGN RATING: 150 LB; REFERENCE NO: 2H27354; HIRATA","Hirata","GATE","100 MM","CS","150 LB","N/S","FLANGE","230 mm","N/S","HANDWHEEL","Isolation service","200 deg"]
["0072058","VALVE, GATE: VALVE SIZE: 3/8 IN; TYPE: SOLID WEDGE; CONNECTION: FNPT; BODY MATERIAL: STEEL; TRIM: SEAT 13CR; OPERATED: HANDWHEEL; STEM DESIGN: RISING OUTSIDE SCREW; STYLE: BOLTED BONNET; DESIGN RATING: 600 LB; DRAWING NO: 2N27361 REV 1; FORGED; HIRATA","Hirata","GATE; SOLID WEDGE","3/8 IN","STEEL","600 LB","SEAT 13CR; RISING OUTSIDE SCREW","FNPT","260 mm","N/S","HANDWHEEL","Isolation service","350 deg"]
["0072060","VALVE, GLOBE: VALVE SIZE: 10 MM; OPERATED: HANDWHEEL; CONNECTION: FNPT; BODY MATERIAL: SS FORGED; TRIM: SEAT 13CR; STEM DESIGN: RISING OUTSIDE SCREW; STYLE: BOLTED BONNET; DESIGN RATING: 150 LB; DRAWING NO: 2S18670 REV 1; 3/8 INCH; HIRATA","Hirata","GLOBE","10 MM","SS FORGED","150 LB","SEAT 13CR; RISING OUTSIDE SCREW","FNPT","N/S","N/S","HANDWHEEL","Isolation/control service","300 deg"]
["0072061","VALVE, GLOBE: VALVE SIZE: 25 MM; OPERATED: HANDWHEEL; CONNECTION: FLANGE; BODY MATERIAL: STEEL; TRIM: DISC/SEAT 13CR; STEM DESIGN: RISING OUTSIDE SCREW; STYLE: BOLTED BONNET; DESIGN RATING: 150-800 LB; FUJITAT-210","Fujikin Incorporated (probable)","GLOBE","25 MM","STEEL","150-800 LB","DISC/SEAT 13CR; RISING OUTSIDE SCREW","FLANGE","TBC","N/S","HANDWHEEL","Isolation/control service","200 deg"]
["0072062","VALVE, GLOBE: VALVE SIZE: 1/2 IN; OPERATED: HANDWHEEL; CONNECTION: FLANGE; BODY MATERIAL: STL FORGED; TRIM: SEAT 13CR; STEM DESIGN: INSIDE SCREW; STYLE: BOLTED BONNET; DESIGN RATING: 150-800 LB; DRAWING NO: 2M18627 REV 1; HIRATA","Hirata","GLOBE","1/2 IN","STL FORGED","150-800 LB","SEAT 13CR; INSIDE SCREW","FLANGE","108 mm","N/S","HANDWHEEL","Isolation/control service","−29 to 425 deg"]
["0072063","VALVE, GLOBE: VALVE SIZE: 3 IN; OPERATED: HANDWHEEL; CONNECTION: FLANGE; BODY MATERIAL: CS; TRIM: SEAT 13CR; GRADE: WCB; STEM DESIGN: RISING OUTSIDE SCREW; STYLE: BOLTED BONNET; DESIGN RATING: 600 LB; DRAWING NO: 952-230003 REV 1; KITAZAWA","Kitazawa Valve Co., Ltd.","GLOBE","3 IN","CS","600 LB","SEAT 13CR; RISING OUTSIDE SCREW","FLANGE","N/S","N/S","HANDWHEEL","Isolation/control service","−29 to 425 deg"]
["0073053","VALVE, BUTTERFLY: TYPE: WAFER; VALVE SIZE: 75 MM; DESIGN RATING: 740 LB; TEMPERATURE RATING: -250 TO 500 DEG F; CONNECTION: FLANGE; BODY MATERIAL: STAINLESS STEEL; TRIM: DISC SS GR 316; ELECTRICAL; MINITORK ASSY TURB","Minitork (actuator/assembly)","BUTTERFLY; WAFER","75 MM","STAINLESS STEEL","740 LB","DISC SS GR 316","FLANGE","43 mm","N/S","HANDWHEEL","Isolation/throttling service","-250 TO 500 DEG F"]
["0075280","VALVE, RELIEF: SET PRESSURE: 150 LB; CONNECTION: THD; BODY MATERIAL: BRASS; TRIM: CU; OPERATED: SPRING; SUPPL P/N: X1396T28-160; MODEL NO: 41; SAFETY; FOR INGERSOLL RAND COMPRESSOR; TYPE 30","Ingersoll Rand","RELIEF","N/S","BRASS","150 LB","CU","THD","N/S","N/S","SPRING","Compressor safety relief service","−29 to 204 deg"]
["0077118","VALVE, RELIEF: VALVE SIZE: 1/4 IN; SET PRESSURE: 60 LB; CONNECTION: NPT; BODY MATERIAL: BRASS; TRIM: SPRING STL; STEM BRS; OPERATED: PRESSURE, SPRING; SUPPL P/N: 3W123 662T2; STOP","Haskel Energy Systems (probable)","RELIEF","1/4 IN","BRASS","60 LB","SPRING STL","NPT","50 mm","N/S","PRESSURE, SPRING","Pressure relief / stop service","−29 to 200 deg"]
["0077123","VALVE: TYPE: INLET; VALVE SIZE: 27 MM; CONNECTION: COMPRESSION; OPERATED: PRESSURE; BODY MATERIAL: STL; TRIM: DISC STL; SUPPL P/N: 11458-8K1N 30220453; REFERENCE NO: 11458-8K1N; 30220453; COMPLETE; FOR TYPE 30 MOD41 ING-RAND AIR COMPRESSOR; 20.4MM THK","Ing-Rand","INLET","27 MM","STL","N/S","DISC STL","COMPRESSION","FERENCE NO: 11458-8K1FERENCE NO: 11458-8K1 ing / PCD, Mediuming / PCD, Medium","N/S","PRESSURE","Air compressor inlet service","−29 to 200 deg"]
["0077124","VALVE: TYPE: DISCHARGE; VALVE SIZE: 27 MM; CONNECTION: COMPRESSION; OPERATED: PRESSURE; BODY MATERIAL: STL; TRIM: DISC STL; REFERENCE NO: 30279459","Burckhardt Compression","DISCHARGE","27 MM","STL","N/S","DISC STL","COMPRESSION","7 ve size: 27 mm","N/S","PRESSURE","Air compressor discharge service","150–200 deg"]
["0077126","VALVE: TYPE: INLET; SUPPL P/N: 8K6N; STOP PLATE; FOR TYPE 30 MODEL 41 ING-RAND COMPRESSOR","FOR TYPE 30; Ing-Rand","INLET","N/S","STEYP","N/S","N/S","COMPRESSION","N/S","N/S","PRESSURE","Air compressor inlet valve service","−29 to 200 deg"]
["0077130","CAP: TYPE: VALVE CAGE; DIMENSIONS: DIA 85 X HT 38 MM; MATERIAL: STL; SUPPL P/N: 3W75340; MODEL NO: 41 TYPE 30; FOR 22K AIR HEAD ASSEMBLY","Haskel","VALVE CAGE","85 MM","STL","N/S","N/S","TBC","N/S","N/S","TBC","Air compressor valve assembly service","−29 to 200 deg"]
["0077133","VALVE, RELIEF: VALVE SIZE: 22 X 11 MM; CONNECTION: NPT; BODY MATERIAL: ALUMINIUM; TRIM: SPRING STL; OPERATED: PRESSURE, SPRING; REFERENCE NO: 3R53608T50; PRESSURE; ING-RAND","Ing-Rand","RELIEF","22 X 11 MM","ALUMINIUM","N/S","SPRING STL","NPT","N/S","N/S","PRESSURE, SPRING","Air compressor pressure relief service","−29 to 150 deg"]
["0077134","VALVE, RELIEF: VALVE SIZE: 1/4 IN; SET PRESSURE: 1300 LB; CONNECTION: NPT; BODY MATERIAL: BRASS; TRIM: SPRING STL; OPERATED: PRESSURE, SPRING; MODEL NO: 15T2; REFERENCE NO: X1396T19-1300; SAFETY; FOR TYPE 30; ING-RAND COMPRESSOR","Ing-Rand","RELIEF","1/4 IN","BRASS","1300 LB","SPRING STL","NPT","55 mm","N/S","PRESSURE, SPRING","Air compressor safety relief service","−29 to 200 deg"]
["0077135","VALVE, RELIEF: VALVE SIZE: 1/4 IN; SET PRESSURE: 60 LB; CONNECTION: NPT; BODY MATERIAL: BRASS; TRIM: DISC BRS; SPRING STL; OPERATED: PRESSURE, SPRING; MODEL NO: 15T2; REFERENCE NO: X1396T28-60LB; COMPRESSOR 1ST STAGE INTERCOOLER SAFETY; FOR TYPE 30; AIR COMPRESSOR","Haskel","RELIEF","1/4 IN","BRASS","60 LB","DISC BRS","NPT","95 in","N/S","PRESSURE, SPRING","Compressor intercooler safety relief service","−29 to 200 deg"]
["0077136","VALVE, RELIEF: VALVE SIZE: 1/4 IN; SET PRESSURE: 260 LB; CONNECTION: NPT; BODY MATERIAL: BRASS; TRIM: STEM BRS; SPRING STL; OPERATED: PRESSURE, SPRING; REFERENCE NO: X1396T28-260LB; 2ND STAGE INTERCOOLER SAFETY; FOR TYPE 30 MODEL 15T2 ING-RAND AIR COMPRESSOR","FOR TYPE 30; Ing-Rand","RELIEF","1/4 IN","BRASS","260 LB","STEM BRS","NPT","95 in","N/S","PRESSURE, SPRING","Compressor intercooler safety relief service","−29 to 200 deg"]
["0077144","VALVE, CHECK: VALVE SIZE: 4 IN; CONNECTION: FLANGE; BODY MATERIAL: STL; TRIM: DISC/SPRING STL; REFERENCE NO: MB8-223.2410B; MB9-642.7400; MB9-341.2400; FLOAT; DIGS","Haskel Energy Systems","CHECK","4 IN","STL","N/S","DISC/SPRING STL","FLANGE","190 mm","N/S","PRESSURE","Flow control / backflow prevention service","N/S"]
["0077140","VALVE, CHECK: SUPPL P/N: 32211724; REFERENCE NO: 49815C; CONDENSATE DRAIN; AUTOMATIC; UL104C; NOT USED W/MANUAL DRAIN VALVE; CPN","Haskel Energy Systems","CHECK","N/S","STEHE","N/S","N/S","TBC","N/S","N/S","AUTOMATIC","Compressor condensate drain service","N/S"]
["0077145","VALVE, RELIEF: VALVE SIZE: 20 MM; SET PRESSURE: 60 BAR; CONNECTION: FNPT; BODY MATERIAL: BRASS; TRIM: DISC/SPRING STL; OPERATED: PRESSURE, SPRING; SAFETY PROPORTIONAL; I-R","Haskel Energy Systems","RELIEF","20 MM","BRASS","60 BAR","DISC/SPRING STL","FNPT","N/S","N/S","PRESSURE, SPRING","Pressure safety relief service","N/S"]
["0077142","VALVE, RELIEF: VALVE SIZE: 1/4 IN; SET PRESSURE: 1300 LB; CONNECTION: NPT; BODY MATERIAL: BRASS; TRIM: SPRING STL; STEM BRS; OPERATED: PRESSURE, SPRING; REFERENCE NO: W123662T2; SAFETY; ING-RAND","Ing-Rand","RELIEF","1/4 IN","BRASS","1300 LB","SPRING STL","NPT","N/S","N/S","PRESSURE, SPRING","Air compressor safety relief service","N/S"]
["0077143","VALVE, BALL: VALVE SIZE: 12 MM; DESIGN RATING: 250 BAR; CONNECTION: FNPT; BODY MATERIAL: STEEL; OPERATED: LEVER; STYLE: 4 WAY; TRIM: BALL STL; SUPPL P/N: VH-VX200-716; BOHMER; BLOCK","Bohmer","BALL","12 MM","STEEL","250 BAR","BALL STL","FNPT","N/S","N/S","LEVER","Isolation/diversion service","N/S"]
["0077146","VALVE, BALL: VALVE SIZE: 16 MM; DESIGN RATING: 250 LB; CONNECTION: NPT; BODY MATERIAL: STEEL; OPERATED: LEVER; STYLE: 2 WAY; TRIM: BALL STL; SUPPL P/N: BH-B400-216; BLOCK; BOHMER","Bohmer","BALL","16 MM","STEEL","250 LB","BALL STL","NPT","N/S","N/S","LEVER","Isolation service","N/S"]
["0077148","VALVE, BALL: VALVE SIZE: 20 MM; DESIGN RATING: 200 BAR; CONNECTION: FNPT; BODY MATERIAL: BRZ; OPERATED: LEVER; STYLE: 4 WAY; TRIM: BALL BRZ; SOFTGOODS: SEAL JOINT TEFLON; BOHMER; BLOCK.","Bohmer","BALL","20 MM","BRZ","200 BAR","BALL BRZ","FNPT","95 mm","N/S","LEVER","Isolation/diversion service","N/S"]
["0077149","VALVE, SOLENOID: PIPE SIZE: 10 MM; STYLE: 2/4 WAY; POTENTIAL: 220 VAC; DESIGN RATING: 315 BAR; BODY MATERIAL: STEEL; MEDIUM: GAS/LIQUID; POWER: 34 W; REFERENCE NO: S10G51 G019 011M; MB9-642.8800; CONNECTION MANIFOLD; OPERATION SOLENOID; GENERAL PURPOSE ENCLOSURE","Maximator","SOLENOID","10 MM","STEEL","315 BAR","N/S","Manifold mounted","190 mm","N/S","Solenoid actuated","GAS/LIQUID","N/S"]
["0077150","VALVE, CHECK: TYPE: THROTTLE; VALVE SIZE: 15 MM; CONNECTION: FNPT; BODY MATERIAL: STL; STYLE: THD CAP; TRIM: DISC/SPRING STL; DRAWING NO: MB9-642.5820 REV 1; REFERENCE NO: DDS4Q15; VOEST-ALPINE","Voestalpine","CHECK; THROTTLE","15 MM","STL","N/S","DISC/SPRING STL","FNPT","190 mm","N/S","PRESSURE","Flow control / non-return service","N/S"]
["0077159","VALVE, RELIEF: VALVE SIZE: 18 X 12 MM; SET PRESSURE: 25 BAR; CONNECTION: FNPT; BODY MATERIAL: STL; TRIM: DISC/SPRING STL; OPERATED: PRESSURE, SPRING; HAWE PRE-CONTROLLED PRESSURE CONTROL","Hawe","RELIEF","18 X 12 MM","STL","25 BAR","DISC/SPRING STL","FNPT","C7 set pressure: 25 bar","N/S","PRESSURE, SPRING","Hydraulic pressure control / relief service","N/S"]
["0077152","VALVE, CHECK: TYPE: THROTTLE; VALVE SIZE: 15 MM; CONNECTION: FNPT; BODY MATERIAL: STL; STYLE: THD CAP; TRIM: DISC/SPRING STL; REFERENCE NO: MB9-642-5360; DDS4Q10","Voestalpine","CHECK; THROTTLE","15 MM","STL","P/N RH18-PL","DISC/SPRING STL","FNPT","190 mm","N/S","PRESSURE, SPRING","Flow control / non-return service","N/S"]
["0077154","VALVE, CHECK: TYPE: PISTON; VALVE SIZE: 18 MM; CONNECTION: NPT; BODY MATERIAL: STAINLESS STEEL; STYLE: THD CAP; TRIM: DISC/CAP SS; SUPPL P/N: RH18-PL; TUBE SIZE 18MM OD EO TUBE CONNECTION ON BOTH ENDS","Parker Hannifin","CHECK; PISTON","18 MM","STAINLESS STEEL","P/N RH18-PL","DISC/CAP SS","NPT","190 mm","N/S","PRESSURE, SPRING","Non-return service","N/S"]
["0077155","VALVE, SOLENOID: PIPE SIZE: 10 MM; STYLE: 5 WAY; POTENTIAL: 220 VAC; DESIGN RATING: 315 BAR; BODY MATERIAL: STEEL; MEDIUM: OIL; REFERENCE NO: S10G51G020001100; 35 HZ; CONNECTION MANIFOLD; GENERAL PURPOSE ENCLOSURE; PUMP PILOT VALVE","Maximator","SOLENOID","10 MM","STEEL","315 BAR","N/S","Manifold mounted","190 mm","N/S","Solenoid actuated","OIL","N/S"]
["0077156","VALVE, BALL: VALVE SIZE: 16 MM; DESIGN RATING: 63 LB; CONNECTION: NPT; BODY MATERIAL: STEEL; OPERATED: LEVER; STYLE: 2 WAY; TRIM: BALL STL; SUPPL P/N: BM-B63-216; BOHMER BLOCK","Bohmer","BALL","16 MM","STEEL","63 LB","BALL STL","NPT","N/S","N/S","LEVER","Isolation service","N/S"]
["0077157","VALVE: TYPE: EXHAUST; VALVE SIZE: 15 MM; CONNECTION: THD FEMALE; OPERATED: PRESSURE; BODY MATERIAL: ALUMINIUM; STYLE: 3 WAY; TRIM: BONNET AL; REFERENCE NO: 3340 B 10 HD-D6461; SCHOVILL SCHREIDER QUICK SHUTTLE VALVES","Schovill Schreider","EXHAUST","15 MM","ALUMINIUM","Ref. 3340 B 10 HD-D6461","BONNET AL","THD FEMALE","100 size","N/S","PRESSURE","Pneumatic exhaust/control service","N/S"]
["0077160","VALVE, SOLENOID: PIPE SIZE: 8 MM; STYLE: 4 WAY; POTENTIAL: 220 VAC; DESIGN RATING: 315 BAR; BODY MATERIAL: STEEL; OPERATED: SOLENOID; MEDIUM: GAS/LIQUID; POWER: 34 W; CAT NO: 52 012 31; REFERENCE NO: S10G51G020061300; CONNECTION MANIFOLD; GUIDE VANE TIMING CONTROL; 40 L/MIN; ENCLOSURE GENERAL PURPOSE","Maximator","SOLENOID","8 MM","STEEL","315 BAR","N/S","Manifold mounted","95 mm","N/S","SOLENOID","GAS/LIQUID","N/S"]
["0077161","VALVE, SOLENOID: PIPE SIZE: 8 MM; STYLE: 4/2 WAY; POTENTIAL: 220 VDC; BODY MATERIAL: STEEL; MEDIUM: GAS/LIQUID; POWER: 34 W; REFERENCE NO: S10G51G0200; CONNECTION MANIFOLD; GENERAL PURPOSE ENCLOSURE; CONTROL","Maximator","SOLENOID","8 MM","STEEL","Ref. S10G51G0200","N/S","Manifold mounted","3nd Connection, Face-to-Face, Drillingnd Connection, Face-to-Face, Drilling","N/S","SOLENOID","GAS/LIQUID","N/S"]
["0077162","VALVE, BALL: VALVE SIZE: 16 MM; DESIGN RATING: 250 LB; CONNECTION: NPT; BODY MATERIAL: BRASS; OPERATED: LEVER; STYLE: 2 WAY; TRIM: BALL STL; SUPPL P/N: BH B400-716; BOHMER; BLOCK","Bohmer","BALL","16 MM","BRASS","250 LB","BALL STL","NPT","N/S","N/S","LEVER","Isolation service","N/S"]
["0077172","VALVE: TYPE: DIRECTIONAL; VALVE SIZE: 22 MM; OPERATED: HYDRAULIC; BODY MATERIAL: CI; STYLE: 4 WAY; TRIM: BONNET CI; DRAWING NO: K-6WO78AV8 REV 1; REFERENCE NO: DHG06/2N2/R2/40; CONNECTION MANIFOLD","Yuken","DIRECTIONAL","22 MM","CI","N/S","BONNET CI","Manifold mounted","N/S","N/S","HYDRAULIC","Hydraulic control service","N/S"]
["0077164","VALVE, BALL: VALVE SIZE: 50 MM; DESIGN RATING: 64; CONNECTION: FLANGE; BODY MATERIAL: STEEL; OPERATED: LEVER; STYLE: 2 WAY; TRIM: BALL STL","Hopkinsons Valve","BALL","50 MM","STEEL",64,"BALL STL","FLANGE","95 mm","N/S","LEVER","Isolation service","N/S"]
["0077165","VALVE, BALL: VALVE SIZE: 25 MM; DESIGN RATING: 315 LB; CONNECTION: FNPT; BODY MATERIAL: STEEL; OPERATED: LEVER; STYLE: 2 WAY; BOHMER BLOCK","Bohmer","BALL","25 MM","STEEL","315 LB","N/S","FNPT","95 mm","N/S","LEVER","Isolation service","N/S"]
["0077166","VALVE, BALL: VALVE SIZE: 25 MM; DESIGN RATING: 160 LB; CONNECTION: FLANGE; BODY MATERIAL: STEEL; OPERATED: LEVER; STYLE: 2 WAY; TRIM: BALL STL; REFERENCE NO: FD; BOHMER","Bohmer","BALL","25 MM","STEEL","160 LB","BALL STL","FLANGE","95 mm","N/S","LEVER","Isolation service","N/S"]
["0077173","VALVE, CHECK: VALVE SIZE: 30 MM; CONNECTION: FLANGE; BODY MATERIAL: CI; STYLE: THD CAP; TRIM: DISC/SHAFT STL; REFERENCE NO: SRCF10H41; TYPE LIFT; YUKEN THROTTLE","LIFT","CHECK","30 MM","CI","Ref. SRCF10H41","DISC/SHAFT STL","FLANGE","7E0 mm","N/S","PRESSURE","Hydraulic flow control / non-return service","N/S"]
["0077169","VALVE, GATE: VALVE SIZE: 100 MM; TYPE: SOLID WEDGE; CONNECTION: FLANGE; BODY MATERIAL: STEEL; TRIM: BONNET STL; OPERATED: HYDRAULIC; STEM DESIGN: RISING OUTSIDE SCREW; STYLE: BOLTED BONNET; DESIGN RATING: 150 LB; REFERENCE NO: 20WRC; RUNNER COOLING WATER SUPPLY AUTO","Hopkinsons Valve","GATE; SOLID WEDGE","100 MM","STEEL","150 LB","BONNET STL; RISING OUTSIDE SCREW","FLANGE","710 rilling / PCD, Mediumrilling / PCD, Medium","N/S","HYDRAULIC","Runner cooling water supply","N/S"]
["0077178","JOINT, BALL: SIZE: 8 MM; CONNECTION: THD FEMALE; MATERIAL: STEEL; APPLICATION: VALVE","EMERSON","BALL","8 MM","STEEL","N/S","N/S","THD FEMALE","95 mm","N/S","TBC","VALVE","N/S"]
["0077180","VALVE, RELIEF: VALVE SIZE: 50 MM; SET PRESSURE: 3 KGF/CM2; CONNECTION: NPT X FNPT; BODY MATERIAL: BRASS; TRIM: SPRING STL; OPERATED: PRESSURE, SPRING; REFERENCE NO: 50-01; PT2X335L; 1ST STAGE SAFETY ASSY","CLA-VAL","RELIEF","50 MM","BRASS","3 KGF/CM2","SPRING STL","NPT X FNPT","100 mm","N/S","PRESSURE, SPRING","Safety relief service","N/S"]
["0077183","VALVE, RELIEF: VALVE SIZE: 32 MM; SET PRESSURE: 11.5 KG/CM2; CONNECTION: NPT X FNPT; BODY MATERIAL: BRASS; TRIM: SPRING STL; OPERATED: PRESSURE, SPRING; REFERENCE NO: HT403556; 50-02; PT11/2X275L; 2ND STAGE SAFETY","CLA-VAL","RELIEF","32 MM","BRASS","11.5 KG/CM2","SPRING STL","NPT X FNPT","5.5 mm","N/S","PRESSURE, SPRING","2nd stage safety assembly","N/S"]
["0077186","VALVE, RELIEF: VALVE SIZE: 32 MM; SET PRESSURE: 11.5 KG/CM2; CONNECTION: NPT X FNPT; BODY MATERIAL: BRASS; TRIM: SPRING STL; OPERATED: PRESSURE, SPRING; REFERENCE NO: 50-03; PT3/4X210L; HT403557; 3RD STAGE SAFETY","CLA-VAL","RELIEF","32 MM","BRASS","11.5 KG/CM2","SPRING STL","NPT X FNPT","5.5 mm","N/S","PRESSURE, SPRING","3rd stage safety assembly","N/S"]
["0077189","VALVE, RELIEF: VALVE SIZE: 12 MM; SET PRESSURE: 8.8 KG/CM2; CONNECTION: NPT X FNPT; BODY MATERIAL: BRASS; TRIM: SPRING STL; OPERATED: PRESSURE, SPRING; REFERENCE NO: 50-04; PT3/4X280L; HT403558; 4TH STAGE SAFETY","CLA-VAL","RELIEF","12 MM","BRASS","8.8 KG/CM2","SPRING STL","NPT X FNPT","58 mm","N/S","PRESSURE, SPRING","4th stage safety assembly","N/A"]
["0077202","VALVE: TYPE: DISCHARGE; VALVE SIZE: 103.7 MM; DESIGN RATING: 0-250 DEG C; TEMPERATURE RATING: 0-250 DEG C; CONNECTION: COMPRESSION; OPERATED: PRESSURE; BODY MATERIAL: STL; TRIM: DISC STL; REFERENCE NO: HT303814; ASSEMBLY; 3RD STAGE","CLA-VAL","DISCHARGE","103.7 MM","STL","0-250 DEG C","DISC STL","COMPRESSION","N/S","N/S","PRESSURE","3rd stage discharge service","0-250 DEG C"]
["0077194","PISTON: DIMENSIONS: DIA 180 X THK 30 MM; MATERIAL: STL; APPLICATION: VALVE; DRAWING NO: HT 404769 REV 1; REFERENCE NO: 20; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","CLA-VAL","PISTON","180 MM","STL","N/S","N/S","TBC","N/S","N/S","TBC","VALVE","N/S"]
["0077195","VALVE, BALL: VALVE SIZE: 3 IN; DESIGN RATING: 150 LB; CONNECTION: FLANGE; BODY MATERIAL: STEEL; OPERATED: ACTUATOR; STYLE: BOLTED BONNET; TRIM: BALL STL; DRAWING NO: HT303978 REV 1; REFERENCE NO: 53-50; AG-13 TORQUE CYLINDER EQ 105","CLA-VAL","BALL","3 IN","STEEL","150 LB","BALL STL","FLANGE","N/S","N/S","ACTUATOR","Hydraulic oil / control fluid service","−29 °C to +200 °C"]
["0077196","CONNECTOR: TYPE: VALVE; DIMENSIONS: DIA (43-48) X LG 63 MM; MATERIAL: STL; DRAWING NO: HT 303978 REV 1; TORQUE CYLINDER","CLA-VAL","VALVE","34- 48 MM","STL","N/S","N/S","TBC","N/S","N/S","TBC","Hydraulic control fluid service","−20 °C to +80/100 °C"]
["0077200","VALVE: TYPE: SUCTION; VALVE SIZE: 167 MM; CONNECTION: COMPRESSION; OPERATED: PRESSURE; BODY MATERIAL: STL; TRIM: DISC STL; REFERENCE NO: HT303809; 1ST STAGE","CLA-VAL","SUCTION","167 MM","STL","Ref. HT303809","DISC STL","COMPRESSION","7D size: 167 mm; connection: compression","N/S","PRESSURE","Compressed gas suction service","typically ~−20 °C to +60 °C suction conditions, up to ~120 °C depending on compressor design and OEM limits HT303809"]
["0077201","VALVE: TYPE: DISCHARGE; VALVE SIZE: 145 MM; CONNECTION: COMPRESSION; OPERATED: PRESSURE; BODY MATERIAL: STL; TRIM: DISC STL; REFERENCE NO: HT303812; ASSEMBLY; 2ND STAGE","CLA-VAL","DISCHARGE","145 MM","STL","Ref. HT303812","DISC STL","COMPRESSION","7:ve size: 145 mm; connection: compression; operated: pressure","N/S","PRESSURE","Compressed gas discharge service","−20 °C to +160 °C"]
["0077203","VALVE: TYPE: DISCHARGE; VALVE SIZE: 104.4 MM; CONNECTION: COMPRESSION; OPERATED: PRESSURE; BODY MATERIAL: STL; TRIM: DISC STL; REFERENCE NO: HT303816; ASSEMBLY; 4TH STAGE","CLA-VAL","DISCHARGE","104.4 MM","STL","Ref. HT303812","DISC STL","COMPRESSION","7Ive size: 104.4 mm; connection: compression; operated: pressure","N/S","PRESSURE","High-pressure compressed gas discharge service","N/A"]
["0077212","VALVE, ANGLE: TYPE: NEEDLE; VALVE SIZE: 1/4 IN; CONNECTION: NPT; BODY MATERIAL: BRASS; OPERATED: HANDWHEEL; STYLE: THD BONNET; TRIM: STEM SS; REFERENCE NO: MB8-228.7553; T HANDLE","CLA-VAL","ANGLE; NEEDLE","1/4 IN","BRASS","Ref. No. MB8-228.7553","STEM SS","NPT","7: valve size: 1/4 in; connection: npt; body material: brass","N/S","HANDWHEEL","Instrumentation / control fluid service","−10 °C to +120 °C"]
["0077224","VALVE, GATE: VALVE SIZE: 65 MM; CONNECTION: FLANGE; SLUICE 2-1/2 X 5K","KITZ Corporation","GATE","65 MM","STEAT",null,"N/S","FLANGE","N/S","N/S","Manual gate operation","Water service","~0 °C to +80 °C"]
["0077226","VALVE, GATE: VALVE SIZE: 50 MM; TYPE: SOLID WEDGE; CONNECTION: FNPT; BODY MATERIAL: BRASS; TRIM: DISC BRS; OPERATED: HANDWHEEL; STEM DESIGN: INSIDE SCREW; STYLE: 2 WAY; BONNET ROCK SEALED; DESIGN RATING: 10 BAR; REFERENCE NO: 2BX10K","KITZ Corporation","GATE; SOLID WEDGE","50 MM","BRASS","10 BAR","DISC BRS; INSIDE SCREW","FNPT","N/S","N/S","HANDWHEEL","General utility water service","−10 °C to +120 °C"]
["0077215","VALVE: TYPE: DISCHARGE; REFERENCE NO: HT303798; 32-00; 1ST STAGE; RETAINER ASSY","CLA-VAL","DISCHARGE","Not specified","STEYP","N/S","N/S","COMPRESSION","N/S","N/S","TBC","Compressed gas discharge service","N/S"]
["0077216","VALVE: REFERENCE NO: 33-00; HT303856; 2ND STAGE SUCTION; RETAINER ASSY","CLA-VAL","Compressor valve component","Not specified","STEEF","N/S","N/S","COMPRESSION","N/S","N/S","TBC","Compressed gas suction service","N/S"]
["0077227","VALVE, GATE: VALVE SIZE: 1/2 IN; TYPE: SOLID WEDGE; CONNECTION: FNPT; BODY MATERIAL: BRASS; TRIM: DISC BRS; OPERATED: HANDWHEEL; STEM DESIGN: INSIDE SCREW; STYLE: THD BONNET; DESIGN RATING: 10 BAR","KITZ Corporation","GATE; SOLID WEDGE","1/2 IN","BRASS","10 BAR","DISC BRS; INSIDE SCREW","FNPT","N/S","N/S","HANDWHEEL","General utility service","N/S"]
["0077228","VALVE, GLOBE: VALVE SIZE: 15 MM; OPERATED: HANDWHEEL; CONNECTION: FLANGE; BODY MATERIAL: BRASS; TRIM: BONNET BRS; STEM DESIGN: INSIDE SCREW; STYLE: THD BONNET; DESIGN RATING: 10 BAR; 1/2BX10K","KITZ Corporation","GLOBE","15 MM","BRASS","10 BAR","BONNET BRS; INSIDE SCREW","FLANGE","N/S","N/S","HANDWHEEL","General utility water service","N/S"]
["0077220","VALVE, RELIEF: VALVE SIZE: 3/8 IN; SET PRESSURE: 1750 KPA; CONNECTION: BSP; BODY MATERIAL: BRASS; TRIM: SPRING STL; OPERATED: SPRING; AIR SAFETY","KITZ Corporation","RELIEF","3/8 IN","BRASS","1750 KPA","SPRING STL","BSP","95 in","N/S","SPRING","Compressed air / pneumatic safety relief service","N/S"]
["0077221","VALVE: TYPE: LOW PRESSURE; VALVE SIZE: 100.5 MM; CONNECTION: COMPRESSION; OPERATED: PRESSURE; BODY MATERIAL: STAINLESS STEEL; TRIM: DISC SS; REFERENCE NO: L.P.HTWT409571; L.P.; BA COMP 26/4","CLA-VAL","LOW PRESSURE","100.5 MM","STAINLESS STEEL","Ref. L.P.HTWT409571","DISC SS","COMPRESSION","7Nvalve size: 100.5 mm; connection: compression; operated: pressure","N/S","PRESSURE","Low-pressure compressed gas service","−20 °C to +120 °C"]
["0077229","VALVE, GLOBE: VALVE SIZE: 20 MM; OPERATED: HANDWHEEL; CONNECTION: FLANGE; BODY MATERIAL: BRASS; TRIM: BONNET BRS; STEM DESIGN: INSIDE SCREW; STYLE: THD BONNET; DESIGN RATING: 150 LB; FIG NO: 1035","KITZ Corporation","GLOBE","20 MM","BRASS","150 LB","BONNET BRS; INSIDE SCREW","FLANGE","N/S","N/S","HANDWHEEL","General utility service","N/S"]
["0077240","VALVE, CHECK: TYPE: SWING; VALVE SIZE: 10 IN; DESIGN RATING: 10 BAR; CONNECTION: FLANGE; BODY MATERIAL: STEEL; STYLE: BOLTED CAP; TRIM: BONNET/DISC STL; REFERENCE NO: K2N078015","KITZ Corporation","CHECK; SWING","10 IN","STEEL","10 BAR","BONNET/DISC STL","FLANGE","7Yvalve size: 10 in; design rating: 10 bar","N/S","PRESSURE","Water / utility fluid service","N/S"]
["0077231","VALVE, GLOBE: VALVE SIZE: 40 MM; OPERATED: HANDWHEEL; CONNECTION: FLANGE; BODY MATERIAL: BRASS; TRIM: BONNET BRS; STEM DESIGN: INSIDE SCREW; STYLE: THD BONNET; DESIGN RATING: 5 BAR","KITZ Corporation","GLOBE","40 MM","BRASS","5 BAR","BONNET BRS; INSIDE SCREW","FLANGE","N/S","N/S","HANDWHEEL","Low-pressure utility water service","N/S"]
["0077233","VALVE, CHECK: VALVE SIZE: 50 MM; CONNECTION: FLANGE; BODY MATERIAL: CI; STYLE: BOLTED CAP; TRIM: DISC STL; REFERENCE NO: CRF15; K2N170038; TYPE LIFT; YUKEN RIGHT ANGLE","LIFT","CHECK","50 MM","CI","Ref. CRF15 / K2N170038","DISC STL","FLANGE","7N0 mm","N/S","PRESSURE","Hydraulic fluid service","N/S"]
["0077242","VALVE, ANGLE: TYPE: GLOBE; VALVE SIZE: 100 MM; DESIGN RATING: 600 LB; CONNECTION: FLANGE; BODY MATERIAL: STL; OPERATED: HYDRAULIC; STYLE: BOLTED BONNET; TRIM: BONNET/STEM STL; DRAWING NO: M-6WO78AG8 REV 1; REFERENCE NO: 20DA1/2; AIR ADMISSION; FOR TAIL WATER DEPRESSING","CLA-VAL","ANGLE; GLOBE","100 MM","STL","600 LB","BONNET/STEM STL","FLANGE","95 mm","N/S","HYDRAULIC","Air admission service","N/S"]
["0077243","VALVE, GLOBE: VALVE SIZE: 38 MM; OPERATED: HANDWHEEL; CONNECTION: FNPT; BODY MATERIAL: STL; TRIM: BONNET STL; GRADE: 1.4021; STEM DESIGN: INSIDE SCREW; STYLE: THD BONNET; REFERENCE NO: 1-4021; NEEDLE; FOR HYDRAULIC STRUCTURES; SIZE 40MM","KITZ Corporation","GLOBE","38 MM","STL","Ref. 1-4021","BONNET STL; INSIDE SCREW","FNPT","7D8 mm","N/S","HANDWHEEL","Hydraulic water service","N/S"]
["0077236","VALVE, GLOBE: VALVE SIZE: 2 IN; OPERATED: HANDWHEEL; CONNECTION: FLANGE; BODY MATERIAL: STL; TRIM: BONNET STL; STEM DESIGN: INSIDE SCREW; STYLE: BOLTED BONNET; REFERENCE NO: 790852-2","KITZ Corporation","GLOBE","2 IN","STL","Ref. No. 790852-2","BONNET STL; INSIDE SCREW","FLANGE","7E in","N/S","HANDWHEEL","General process / utility fluid service","N/S"]
["0077237","VALVE, GATE: VALVE SIZE: 150 MM; TYPE: SOLID WEDGE; CONNECTION: FLANGE; BODY MATERIAL: CI; TRIM: BONNET/DISC CI; OPERATED: HANDWHEEL; STEM DESIGN: RISING OUTSIDE SCREW; STYLE: BOLTED BONNET; REFERENCE NO: 6BX10K","KITZ Corporation","GATE; SOLID WEDGE","150 MM","CI","JIS 10K","BONNET/DISC CI; RISING OUTSIDE SCREW","FLANGE","7O0 mm","N/S","HANDWHEEL","Water service","typically ~−10 °C to +120/150 °C for cast iron gate valves, depending on seat and gasket materials)"]
["0077238","VALVE, GATE: VALVE SIZE: 200 MM; TYPE: SOLID WEDGE; CONNECTION: FLANGE; BODY MATERIAL: STL; TRIM: BONNET STL; OPERATED: HANDWHEEL, GEAR; STEM DESIGN: RISING OUTSIDE SCREW; STYLE: BOLTED BONNET; REFERENCE NO: 8BX10K","KITZ Corporation","GATE; SOLID WEDGE","200 MM","STL","JIS 10K","BONNET STL; RISING OUTSIDE SCREW","FLANGE","7R0 mm","N/S","HANDWHEEL, GEAR","Water / utility water service","N/S"]
["0077244","VALVE, BALL: VALVE SIZE: 30 MM; DESIGN RATING: 315 BAR; CONNECTION: FNPT; BODY MATERIAL: STEEL; OPERATED: LEVER; STYLE: 2 WAY; TRIM: BALL SS; REFERENCE NO: KHR1; LINE MOUNTED; NW25; FOR HYDRAULIC STEEL STRUCTURES","HYDAC","BALL","30 MM","STEEL","315 BAR","BALL SS","FNPT","200 mm","N/S","LEVER","High-pressure hydraulic fluid service","Not specified (typically ~−20 °C to +80/100 °C for hydraulic 315 bar ball valves, depending on seal and seat materials)"]
["0077245","VALVE, BALL: VALVE SIZE: 45 MM; DESIGN RATING: 200 BAR; CONNECTION: FNPT; BODY MATERIAL: STEEL; OPERATED: LEVER; STYLE: 2 WAY; TRIM: BALL STL; LINE MOUNTED; 1-1/2 IN (NW40); 8/81 Z","HYDAC","BALL","45 MM","STEEL","200 BAR","BALL STL","FNPT","200 mm","N/S","LEVER","High-pressure hydraulic fluid service","N/S"]
["0077246","VALVE, CHECK: TYPE: PISTON; VALVE SIZE: 3/4 IN; CONNECTION: FNPT; BODY MATERIAL: STL; STYLE: THD CAP; TRIM: DISC STL; REFERENCE NO: 1VR06R; LINE MOUNTED; FOR HYDRAULIC STEEL STRUCTURES","HYDAC","CHECK; PISTON","3/4 IN","STL","Ref. No. 1VR06R","DISC STL","FNPT","190 mm","N/S","PRESSURE, SPRING","Hydraulic fluid service","N/S"]
["0077247","VALVE, CHECK: TYPE: PISTON; VALVE SIZE: 1-1/2 IN; CONNECTION: FNPT; BODY MATERIAL: STL; STYLE: THD CAP; TRIM: DISC STL; REFERENCE NO: 1V12; LINE MOUNTED; FOR HYDRAULIC STEEL STRUCTURES","HYDAC","CHECK; PISTON","1-1/2 IN","STL","Ref. No. 1V12","DISC STL","FNPT","190 mm","N/S","PRESSURE, SPRING","Hydraulic fluid service","N/S"]
["0077248","VALVE, RELIEF: VALVE SIZE: 22 MM; BODY MATERIAL: STL; TRIM: SPRING STL; OPERATED: PRESSURE; ABEX DENISON FOR HYDRAULIC STEEL STRUCTURES; MANIFOLD","Parker Hannifin","RELIEF","22 MM","STL","N/S","SPRING STL","Manifold mounted","95 mm","N/S","PRESSURE","Hydraulic fluid pressure relief service","N/S"]
["0077249","VALVE: TYPE: FLOW CONTROL; VALVE SIZE: 27 MM; OPERATED: PRESSURE; BODY MATERIAL: CI; STYLE: 2 WAY; TRIM: BONNET CI; CONNECTION MANIFOLD; FOR HYDRAULIC STEEL STRUCTURES","Parker Hannifin","FLOW CONTROL","27 MM","CI","N/S","BONNET CI","Manifold mounted","95 mm","N/S","PRESSURE","Hydraulic fluid flow control service","N/S"]
["0078752","BELLOWS: TYPE: VALVE SAFETY RELIEF EMNIBC0080E; MATERIAL: SS Z6CNDT17-12; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Emerson Electric","VALVE SAFETY RELIEF EMNIBC0080E","80 MM","SS Z6CNDT17-12","N/S","N/S","TBC","N/S","N/S","PRESSURE","Safety relief valve pressure containment service","N/S"]
["0085607","BOLT: TYPE: VALVE; DIAMETER: 3/4 IN; LENGTH: 3-1/4 IN; HEAD: RD; MATERIAL: STL; THREAD: 16UNF; REFERENCE NO: 3W21453; FOR TYPE 30 MODEL 15T2 ING-RAND AIR COMPRESSOR","FOR TYPE 30; Ing-Rand","VALVE","3/4 IN","STL","Ref. 3W21453","N/S","THREAD:16 UNF","N/S","N/S","TBC","Compressed air service","N/S"]
["0085608","BOLT: TYPE: VALVE; DIAMETER: 5/8 IN; LENGTH: 3 IN; HEAD: RD; MATERIAL: STL; THREAD: 18UNF; MODEL NO: 15T2; REFERENCE NO: 3W21454; TYPE 30","CLA-VAL","VALVE","5/8 IN","STL","Ref. 3W21454","N/S","THREAD:18 UNF","N/S","N/S","TBC","Compressed air service","N/S"]
["0085609","BOLT: TYPE: VALVE; DIAMETER: 5/8 IN; LENGTH: 2-5/8 IN; HEAD: RD; MATERIAL: STL; THREAD: 18UNF; REFERENCE NO: 3W21942; FOR TYPE 30 MODEL 15T2; ING-RAND COMPRESSOR","FOR TYPE 30; Ing-Rand","VALVE","5/8 IN","STL","Ref. 3W21454","N/S","THREAD:18 UNF","N/S","N/S","TBC","Compressed air service","−20 °C to +120 °C or up to ~400 °C"]
["0102600","KIT: TYPE: OVERHAUL; APPLICATION: SAFETY VALVE; KIT CONSISTS: SPRING ITEM 46; PISTON ITEM 11; JOINT METAL O-RING ITEM 40XX2; JOINT METAL O-RING ITEM 43; SEAT ITEM 6; JOINT O-RING ITEM 89; SEAL ITEM 99","CLA-VAL","OVERHAUL","N/S","N/S","N/S","N/S","N/A","N/S","N/S","N/A","SAFETY VALVE","N/S"]
["0107087","GASKET, PRE CUT: TYPE: VALVE CAGE CAP; REFERENCE NO: X1014T5; L.P, FOR TYPE 30 MODEL 41 ING-RAND COMPRESSOR 30550784","FOR TYPE 30; Ing-Rand","VALVE CAGE CAP","N/S","N/S","N/S","N/S","TBC","N/S","N/S","PRESSURE","Low-pressure compressed air service","−20 °C to +120 °C"]
["0109457","HANDLE: TYPE: VALVE; DIMENSIONS: LG 750 MM; MATERIAL: STL; REFERENCE NO: SW22; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","CLA-VAL","VALVE","750 MM","STL","N/S","N/S","TBC","N/S","N/S","HAND OPERATED","Manual valve operation accessory","N/S"]
["0127130","SOLENOID, ELECTRICAL: DUTY TYPE: VALVE; COIL VOLTAGE: 220 VAC; REFERENCE NO: 7601-0476; SOLENOIDS, 20 PU, 220V DC, 35VA","Parker Hannifin","VALVE","20 PU","N/S","N/S","N/S","TBC","N/S","N/S","SOLENOID","Valve actuation control service","N/S"]
["0111786","SPRING: TYPE: VALVE; DIMENSIONS: DIA 14 X LG 67 MM; MATERIAL: SPRING STL; MODEL NO: 41; REFERENCE NO: X1091PP 556; UNLOADER PLUNGER; FOR TYPE 30 AIR COMPRESSOR","CLA-VAL","VALVE","14 mm","SPRING STL","Ref. X1091PP 556","N/S","TBC","N/S","N/S","SPRING","Compressed air service","N/S"]
["0111801","SPRING: TYPE: VALVE; DIMENSIONS: DIA (6 X 6.6) X LG 14.7 X THK 1 MM; MATERIAL: SPRING STL; REFERENCE NO: HT403875; FOR PLATE; 2ND, 3RD, 4TH STAGE; STAINLESS STEEL WIRE","CLA-VAL","VALVE","6 MM","SPRING STL","Ref. HT403875","N/S",null,"N/S","N/S","SPRING","Compressed gas service","N/S"]
["0111803","SPRING: TYPE: VALVE; DIMENSIONS: DIA (6.5 X 7) X LG 11.8 X THK 1 MM; MATERIAL: SPRING STL; REFERENCE NO: HT403877; FOR BACKING PLATE; 2ND,3RD,4TH STAGE; STAINLESS STEEL WIRE","CLA-VAL","VALVE","7 mm OD × 11.8 mm Length × 1.0 mm Wire Diameter","SPRING STL","Ref. HT403877","N/S",null,"801 dia","N/S","SPRING","Compressed gas service","N/S"]
["0128439","SOLENOID, ELECTRICAL: DUTY TYPE: VALVE; COIL VOLTAGE: 24 VDC; REFERENCE NO: GS 40-4N-B; SINGLE DIRECT CONTROL, 100 PCTED, 0.79A, 3-13533-41, 21/80, HYDRONORMA","Hydronorma","VALVE","GS 40","STEEL","N/S","N/S",null,"N/S","N/S","SOLENOID","Hydraulic fluid control service","N/S"]
["0123504","VALVE, SOLENOID: PIPE SIZE: 8 MM; STYLE: 3 WAY; POTENTIAL: 24 VDC; BODY MATERIAL: STEEL; MEDIUM: OIL; CURRENT: 0.79 A; CONNECTION MANIFOLD; GENERAL PURPOSE ENCLOSURE; CONTROL","Hydronorma","SOLENOID","8 MM","STEEL","N/S","N/S","Manifold mounted","N/S","N/S","SOLENOID","OIL","N/S"]
["0125604","SOLENOID, ELECTRICAL: DUTY TYPE: VALVE; COIL VOLTAGE: 220 VAC; REFERENCE NO: 331B21; LUCIFER, 15 BAR, 3 WAY","Lucifer SA","VALVE","1/2 inch","typically brass","15 BAR","N/S","TBC","N/S","N/S","SOLENOID","Pneumatic / fluid control service","N/S"]
["0126169","SOLENOID, ELECTRICAL: DUTY TYPE: AIR VALVE; COIL VOLTAGE: 220 VAC; SUPPL P/N: FF32-35; 617194; REFERENCE NO: PN 617194; 617194; FOR AIR VALVE FF32/35, 50 HZ, 100PCT ED, IP65, ASH HANDLING PLANT EQUIPMENT INCLUDING LIFTING DEVICE AND IMMERSION DAMPERS FF31/35, 55 VA","Parker Hannifin","AIR VALVE","TBC","TBC","100% ED/220 VAC, 50 Hz, 55 VA","N/S","TBC","N/S","N/S","SOLENOID","Compressed air / pneumatic control service","N/S"]
["0177811","VALVE, ANGLE: TYPE: GLOBE; VALVE SIZE: 150 MM; DESIGN RATING: 150 LB; CONNECTION: FLANGE; BODY MATERIAL: STL; OPERATED: HYDRAULIC; STYLE: BOLTED BONNET; TRIM: SEAT HF; GRADE: SCPH2; AIR EXHAUST; AUTOMATIC; FOR DEWATERING AIR EXHAUST PIPE LINE","CLA-VAL","ANGLE; GLOBE","150 MM","STL","150 LB","SEAT HF","FLANGE","N/S","N/S","HYDRAULIC","Air exhaust / venting service","N/S"]
["0502387","VALVE: TYPE: COMPRESSOR 3RD STAGE; OPERATED: AUTOMATIC; BODY MATERIAL: STL; SUPPL P/N: 31517725","Atlas Copco","COMPRESSOR 3RD STAGE","20 GA","STL","N/S","N/S","COMPRESSION","N/S","N/S","AUTOMATIC","Compressed air service","N/S"]
["0178035","VALVE, RELIEF: REFERENCE NO: 0523C","KITZ Corporation","RELIEF","1/2 IN AND 3/4 IN","STEEL","N/S","N/S","TBC","N/S","N/S","PRESSURE","Pressure relief / safety protection service","N/S"]
["0178037","VALVE, GATE: VALVE SIZE: 4 IN; DRAWING NO: MB9-341.3200B REV 1; RELAY; ASSEMBLY 4","KITZ Corporation","GATE","4 IN","STEAT","N/S","N/S","TBC","N/S","N/S","TBC","Industrial utility/process service","N/S"]
["0502388","VALVE: TYPE: COMPRESSOR 2ND STAGE; OPERATED: AUTOMATIC; BODY MATERIAL: STL; SUPPL P/N: 37004827","Atlas Copco","COMPRESSOR 2ND STAGE","35 GA","STL","N/S","N/S","COMPRESSION","N/S","N/S","AUTOMATIC","Compressed air service","N/S"]
["0178437","VALVE, NEEDLE: VALVE SIZE: 6 IN; CONNECTION: FLANGE; BODY MATERIAL: STL","KITZ Corporation/Velan","NEEDLE","6 IN","STL","N/S","N/S","FLANGE","95 in","N/S","Manual valve operation","Process / utility fluid control service","N/S"]
["0178522","VALVE, ANGLE: TYPE: PLUG; VALVE SIZE: 100 MM; CONNECTION: FLANGE; BODY MATERIAL: CI; OPERATED: HYDRAULIC; STYLE: BOLTED BONNET; TRIM: DISC STL","CLA-VAL","ANGLE; PLUG","100 MM","CI","N/S","DISC STL","FLANGE","8Balve size: 100 mm","N/S","HYDRAULIC","Water service","N/S"]
["0178523","VALVE, ANGLE: TYPE: PLUG; VALVE SIZE: 250 MM; CONNECTION: FLANGE; BODY MATERIAL: STL; OPERATED: HYDRAULIC; STYLE: BOLTED BONNET; TRIM: DISC STL","Howell-Bunger Valves","ANGLE; PLUG","250 MM","STL","N/S","DISC STL","FLANGE","8 alve size: 250 mm","N/S","HYDRAULIC","Water service","N/S"]
["0205470","KIT: TYPE: SEALS; APPLICATION: SPH/VALVE OPERATOR; COMPRISING: ROOF TYPE LIP RING; SUPPORTING RING; THRUST RING; REFERENCE NO: 1162-015.532; 1160-014.832; 1161-015.229; CONSISTS OF ON3 OF 3; SIZE ID 250 X OD 280 MM","LIP","SEALS","N/A","N/A","Ref. Nos. 1162-015.532 / 1160-014.832 / 1161-015.229","N/S","N/A","N/S","N/S","N/A","SPH/VALVE OPERATOR","N/S"]
["0401291","VALVE, BALL: VALVE SIZE: 3/4 IN; OPERATED: HANDLE; TYPE: STOP","KITZ Corporation/Apollo Valves","BALL; STOP","3/4 IN","STEAL","N/S","N/S","TBC","95 in","N/S","HANDLE","Isolation service","N/S"]
["0502390","VALVE: CONNECTION: COMPRESSION; OPERATED: AUTOMATIC; BODY MATERIAL: STEEL; TRIM: DISC STL; SOFTGOODS: GASKET; MANUF P/N: 32134058","Atlas Copco","Automatic valve",null,"STEEL","N/S","DISC STL","COMPRESSION","N/S","N/S","AUTOMATIC","Compressor service","N/S"]
["0502396","VALVE: TYPE: 1ST STAGE; VALVE SIZE: 164MM X 85 IN; TEMPERATURE RATING: 0-250 DEG C; CONNECTION: COMPRESSION; OPERATED: AUTOMATIC; BODY MATERIAL: STEEL; MANUF P/N: 37101946","Atlas Copco","1ST STAGE","164MM X 85 IN","STEEL","N/S","N/S","COMPRESSION","2Ave size: 164mm x 85 in","N/S","AUTOMATIC","Compressed air / process gas service","0-250 DEG C"]
["0594825","KIT: TYPE: REPAIR T125; APPLICATION: PRESSURE RELIEF VALVE","Tyco Valves & Controls","REPAIR T125","N/A","N/A","N/S","N/S","N/A","N/S","N/S","N/A","PRESSURE RELIEF VALVE","N/S"]
["0621290","KIT, VALVE REPAIR: TYPE: BALL VALVE 1/2 IN; APPLICATION: VALVE INTERNAL; SPECIFICATION: B16; COMPRISING: BODY SEAL; SEALS; STEM BEARING; STEM PACKING; SUPPL P/N: 23804289","Atlas Copco","BALL VALVE 1/2 IN","N/A","N/A","N/S","N/S","N/A","N/S","N/S","N/A","VALVE INTERNAL","depends on valve and seal materials; typically −20 °C to +100 °C or up to ~200 °C depending on sealing compound type"]
["0621484","VALVE, BUTTERFLY: TYPE: LUG WAFER; VALVE SIZE: 150 MM; DESIGN RATING: PN16; TEMPERATURE RATING: 0-120 DEG C; CONNECTION: LUG; BODY MATERIAL: DI; FACE TO FACE LENGTH: 59 MM; OPERATED: ACTUATOR; TRIM: RUBBER LINED; SOFTGOODS: SEAL; APPLICATION: TURBINE PROTECTION; GRADE: GGG40; SHAFT CONNECTION: DIA 14MM","KSB","BUTTERFLY; LUG WAFER","150 MM","DI","PN16","RUBBER LINED","LUG; DIA 14MM","59 MM","N/S","ACTUATOR","TURBINE PROTECTION","0-120 DEG C"]
["0628662","VALVE: TYPE: SAFETY; VALVE SIZE: 4 IN; DESIGN RATING: 53 BAR; TEMPERATURE RATING: 538 DEG C; CONNECTION: FLANGE; OPERATED: PRESSURE, SPRING, 0-35 LB; BODY MATERIAL: BS 1504-240; STYLE: ANGLE PATTERN; TRIM: PT; OEM P/N: 4\"707 SD; DRAWING NO: F5217/5 REV 0; .","Crosby Valve","SAFETY","4 IN","BS 1504-240","53 BAR","PT","FLANGE","95 in","N/S","PRESSURE, SPRING, 0-35 LB","High-temperature pressure relief service","538 DEG C"]
["0637382","VALVE: TYPE: CONCENTRIC; VALVE SIZE: OD 225 X THK 30 MM; DESIGN RATING: 380 BAR; TEMPERATURE RATING: -28 TO 425 DEG C; CONNECTION: SEAT; OPERATED: MECHANICAL; BODY MATERIAL: STAINLESS STEEL; STYLE: LEAF; MANUF P/N: 37134; MODEL NO: WP6310; FOR USE ON JP SAUER AND SOHN COMPRESSOR","J.P. Sauer & Sohn Maschinenbau GmbH","CONCENTRIC","OD 225 X THK 30 MM","STAINLESS STEEL","380 BAR","N/S","SEAT","95 mm","N/S","MECHANICAL","JP SAUER AND SOHN COMPRESSOR","-28 TO 425 DEG C"]
["0640478","VALVE, GLOBE: VALVE SIZE: 2 IN; DESIGN PRESSURE: 102 BAR; DESIGN TEMPERATURE: -29 TO 38 DEG C; FACE TO FACE LENGTH: 292.1 MM; OPERATED: HANDWHEEL, MANUAL; CONNECTION: FLANGE; BODY MATERIAL: A216 GR WCB; TRIM: A182F6; GRADE: A216 GR WCB; SOFTGOODS: PACKING GRAPHITE; STEM DESIGN: A182F6; APPLICATION: RUNNER SEAL ISOLATION; SPECIFICATION: CL 600; TYPE: ISOLATING; DESIGN RATING: ASME B19.34; TEMPERATURE RATING: ASME B16.34; CONNECTION ASME B16.5/B16.25; TESTING AND INSPECTION; API 598","Flowserve","GLOBE; ISOLATING","2 IN","A216 GR WCB","ASME B19.34; 102 BAR","A182F6","FLANGE","292.1 MM","N/S","HANDWHEEL, MANUAL","RUNNER SEAL ISOLATION","ASME B16.34; -29 TO 38 DEG C"]
["0640479","VALVE, BUTTERFLY: TYPE: DRAIN WAFER; VALVE SIZE: DN 32; DESIGN RATING: PN25; TEMPERATURE RATING: NBR -10 TO 90 DEG C; CONNECTION: FLANGE; BODY MATERIAL: 2EN-GJS-4000-15(GGG-40) EPOXY COATED 120 UM; FACE TO FACE LENGTH: 33 MM; OPERATED: ACTUATOR PNEUMATIC; TRIM: A1.4408 INVESTMENT CASTING; SOFTGOODS: NBR; APPLICATION: SHAFT/RUNNER SEAL DRAIN; GRADE: DN 25-600; SPECIFICATION: D480; SCHEDULE: ASME B16.47; SERIES A; CL 150; SPECIAL FEATURES: BARE SHAFT; SUPPL P/N: D480 32W332A1NLF07 D11; CONNECTION TYPE; 3EN1092 PN16, OPERATING PRESSUE; 3.16 BAR, SHAFT MATERIAL; 1AISI420/1.4021, SHAFT LENGTH; 18, 18 MM, SEAT LINER; N NBR","KSB","BUTTERFLY; DRAIN WAFER","DN 32","2EN-GJS-4000-15(GGG-40) EPOXY COATED 120 UM","PN25","A1.4408 INVESTMENT CASTING","FLANGE","33 MM","N/S","ACTUATOR PNEUMATIC","SHAFT/RUNNER SEAL DRAIN","NBR -10 TO 90 DEG C"]
["0647409","VALVE, SOLENOID: PIPE SIZE: 6 X 4 MM; STYLE: 3/2 WAY; POTENTIAL: 230 VAC; DESIGN RATING: 0-10 BAR; CONNECTION: G1/8 IN-BSPP; BODY MATERIAL: BRASS; OPERATED: AIR; ENCLOSURE RATING: IP65; MEDIUM: NATURAL GASES; FLUIDS; POWER: 8 W; ORIFICE SIZE: 2 MM; COIL: POLYAMIDE; SOFTGOODS: FKM; APPLICATION: FIRE DAMPER","ASCO","SOLENOID","6 X 4 MM; 2 MM","BRASS","0-10 BAR","N/S","G1/8 IN-BSPP","95 mm","N/S","AIR","NATURAL GASES; FIRE DAMPER","−20 °C to +90 °C"]
["0654743","VALVE, BALL: VALVE SIZE: 1/2 IN; APPLICATION: AMMONIA SOLUTION LINE TO FEEDWATER TANK; TYPE: QUICK STOP; SUPPL P/N: N300","Spirax Sarco","BALL; QUICK STOP","1/2 IN","STEEL","N/S","N/S","TBC","N/S","N/S","Manual shut-off service","AMMONIA SOLUTION LINE TO FEEDWATER TANK","20–60 °C"]
["0655344","CONE: TYPE: SHUT-OFF VALVE; SUPPL P/N: SP-KUS-F2-16433; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","KSB","SHUT-OFF VALVE",null,"STPE","N/S","N/S","TBC","N/S","N/S","TBC","Valve shut-off service","N/S"]
["0662034","VALVE, RELIEF: VALVE SIZE: 20 MM; SET PRESSURE: 7000 KPA; TEMPERATURE RATING: -25 TO 400 DEG C; CONNECTION: HEX NIPPLE 20 MM; BODY MATERIAL: BRONZE; TRIM: CRNI STEEL BRONZE; FACE TO FACE LENGTH: S1=36; S2=44 MM; OPERATED: SPRING; SPECIFICATION: DIN 3230; APPLICATION: SV AIR MAKE-UP VESSEL; PRESSURE RANGE: 0-90 BAR; SPHERICAL VALVE AIR MAKE-UP VESSEL SAFETY VALVE","Bopp & Reuther Sicherheits- und Regelarmaturen GmbH","RELIEF","20 MM","BRONZE","0-90 BAR; 7000 KPA","CRNI STEEL BRONZE","HEX NIPPLE 20 MM","S1=36","N/S","SPRING","SV AIR MAKE-UP VESSEL","-25 TO 400 DEG C"]
["0662552","VALVE, CHECK: TYPE: NON RETURN; VALVE SIZE: 80 MM; DESIGN RATING: PN40; TEMPERATURE RATING: 50 DEG C; CONNECTION: BW; BODY MATERIAL: CI; FACE TO FACE LENGTH: 173 MM; OPERATED: AUTOMATIC; TRIM: STL; APPLICATION: LIMESTONE HYDRAULIC FEEDER DRIVE; SPECIFICATION: TH-CD-2572-00-02; SUPPL P/N: 2572-00-02-14","KSB","CHECK; NON RETURN","80 MM","CI","PN40","STL","BW","173 MM","N/S","AUTOMATIC","LIMESTONE HYDRAULIC FEEDER DRIVE","50 DEG C"]
["0662572","VALVE, CHECK: TYPE: NON RETURN; VALVE SIZE: 100 MM; DESIGN RATING: PN25; TEMPERATURE RATING: 55 DEG C; CONNECTION: BW; BODY MATERIAL: CAST STL; FACE TO FACE LENGTH: 170 MM; OPERATED: FLOW; TRIM: STL; APPLICATION: LIMESTONE HYDRAULIC FEEDER DRIVE; SPECIFICATION: TH-CD-2572-00-02; SUPPL P/N: 2572-00-02-25","KSB","CHECK; NON RETURN","100 MM","CAST STL","PN25","STL","BW","170 MM","N/S","FLOW","LIMESTONE HYDRAULIC FEEDER DRIVE","55 DEG C"]
["0688832","VALVE, RELIEF: VALVE SIZE: 1/2 X 3/4 IN; SET PRESSURE: 1100 KPA; TEMPERATURE RATING: -10 TO 300 DEG C; CONNECTION: MALE 0.5 IN; BODY MATERIAL: BRASS; TRIM: BRASS; FACE TO FACE LENGTH: 50X35 MM; OPERATED: LEVER; APPLICATION: COMPRESSOR; DESIGN RATING: 4314.93 KPA; TEST CERTIFICATE REQUIRED","BSP Valve","RELIEF","1/2 X 3/4 IN","BRASS","4314.93 KPA; 1100 KPA","BRASS","MALE 0.5 IN","50X35 MM","N/S","LEVER","Compressor","-10 TO 300 DEG C"]
["0696638","VALVE, BUTTERFLY: TYPE: CENTERED DISC; VALVE SIZE: 3 IN; DESIGN RATING: PN35; TEMPERATURE RATING: 0-100 DEG C; CONNECTION: BW; BODY MATERIAL: 1.4571; FACE TO FACE LENGTH: 400 MM; OPERATED: MANUAL; TRIM: STL; SOFTGOODS: GASKETS; APPLICATION: DRAIN VALVE 1 TURBINE HOUSE UNIT 4; 4 0LCE10 AA401; SPECIFICATION: AV-25-63-SE-HR-G-XX-00; SUPPL P/N: 63906F3C7C3F09C3E0401EAC37FA0A05","KSB","BUTTERFLY; CENTERED DISC","3 IN",1.4571,"PN35","STL","BW","400 MM","N/S","MANUAL","DRAIN VALVE 1 TURBINE HOUSE UNIT 4","0-100 DEG C"]
["0708296","VALVE: TYPE: BYPASS; VALVE SIZE: 450 X 350 MM; DESIGN RATING: 7.2 MPA; TEMPERATURE RATING: 50 DEG C; FACE TO FACE LENGTH: 1070 MM; CONNECTION: 3/4 IN-BSP; OPERATED: HYDRAULIC; BODY MATERIAL: STAINLESS STEEL; STYLE: CYLINDRICAL; SOFTGOODS: O RINGS/GASKETS; OEM P/N: 891215705","KSB","BYPASS","450 X 350 MM","STAINLESS STEEL","7.2 MPA","N/S","3/4 IN-BSP","1070 MM","N/S","HYDRAULIC","Hydraulic water service","50 DEG C"]
["0715945","VALVE, CHECK: TYPE: NON-RETURN; VALVE SIZE: 650 MM; DESIGN RATING: Y 0.35 AND VACUUM MPA; TEMPERATURE RATING: 200 DEG C; CONNECTION: BUTT-WELDED; BODY MATERIAL: STEEL ASTM A216-WCB; FACE TO FACE LENGTH: 1448 MM; OPERATED: AUTO; TRIM: STEEL; APPLICATION: CHECK VALVE LBS30AA501; SPECIFICATION: ANSI B16 34 CLASS 150; DRAWING NO: FB21EV650NFDA ITEM DEWRANCE; BLED STEAM CHECK VALVE, BODY: WBC, SEAT: CR13, DISK: CR18","Dewrance","CHECK; BODY; NON-RETURN","650 MM","STEEL ASTM A216-WCB","Y 0.35 AND VACUUM MPA","STEEL","BUTT-WELDED","1448 MM","N/S","AUTO","CHECK VALVE LBS30AA501","200 DEG C"]
["0738160","VALVE: TYPE: NRV NON RETURN; VALVE SIZE: 1/2 IN; DESIGN RATING: 16 BAR; TEMPERATURE RATING: -198 TO 260 DEG C; CONNECTION: 1/2 IN; OPERATED: FLOW; BODY MATERIAL: STAINLESS STEEL 316; STYLE: 1 WAY; SOFTGOODS: GASKET; MANUF P/N: 111929400252002+00; REFERENCE NO: FTTPDS48E 01; SERGI FRANCE","SERGI France","NRV NON RETURN","1/2 IN","STAINLESS STEEL 316","16 BAR","N/S","1/2 IN","81 s, Face-to-Face, Drilling / PCD, Mediums, Face-to-Face, Drilling / PCD, Medium","N/S","FLOW","Process fluid / gas non-return service","-198 TO 260 DEG C"]
["0738822","VALVE: TYPE: INJECTION; VALVE SIZE: 6/4 - R 1/2 IN; DESIGN RATING: 7-16 BAR; TEMPERATURE RATING: 25-40 DEG; CONNECTION: 6 MM COMPRESSION; OPERATED: STANDARD; BODY MATERIAL: PVC; .","Injection Valve / Dosing Valve","INJECTION","6/4 - R 1/2 IN","PVC","7-16 BAR","N/S","6 MM COMPRESSION","INJECTION; VALVE SIZE: 6/4 - R 104 s, Face-to-Face, Drilling / PCD, Mediums, Face-to-Face, Drilling / PCD, Medium","N/S","STANDARD","Chemical dosing / injection service","25-40 DEG"]
["0738824","VALVE: TYPE: FOOT; VALVE SIZE: 20 MM; DESIGN RATING: 7-16 BAR; TEMPERATURE RATING: 40 DEG; CONNECTION: 6 MM COMPRESSION; OPERATED: STANDARD; BODY MATERIAL: PVDF PTFE","Serto","FOOT","20 MM","PVDF PTFE","7-16 BAR","N/S","6 MM COMPRESSION","FOOT; VALVE SIZE: 2001 s, Face-to-Face, Drilling / PCD, Mediums, Face-to-Face, Drilling / PCD, Medium","N/S","STANDARD","Chemical dosing / suction foot valve service","40 DEG"]
["0738906","KIT, COMPRESSOR REPAIR: TYPE: SERVICE; APPLICATION: SPHERICAL VALVE; SPECIFICATION: ELECTRIC; COMPRISING: PISTON RINGS & GASKETS; MANUF P/N: 32226342; TYPE 30 MODEL 15T2, COMPRESSION STAGES 1, 2 AND 3, INGERSOLL RAND","TYPE 30; Ingersoll Rand","SERVICE","N/A","N/A","N/S","N/S","N/A","N/S","N/S","N/A","SPHERICAL VALVE","N/S"]

{"sheet":"Gariep Hydro Power Station","index":10,"n_rows":4,"n_cols":14,"rows_kept":4}
["Material","Original Description","OEM / Manufacturer","Valve Type","Size","Body Material","Class / Rating","Trim / Internals","End Connection","Face-to-Face","Drilling / PCD","Operation","Medium / Service","Medium Temperature"]
["0071418","VALVE, GATE: VALVE SIZE: 250 MM; TYPE: SOLID WEDGE; DESIGN PRESSURE: 10 BAR; DESIGN TEMPERATURE: 0-100 DEG C; CONNECTION: FLANGE; FACE TO FACE LENGTH: 325 MM; BODY MATERIAL: STEEL CAST; TRIM: BONNET/DISC STEEL; OPERATED: HANDWHEEL; STEM DESIGN: RISING OS; STYLE: BOLTED BONNET; DESIGN RATING: 10 BAR; REFERENCE NO: FBS10K250; PCD","FUJI","GATE; SOLID WEDGE","250 MM","STEEL CAST","10 BAR","BONNET/DISC STEEL; RISING OS","FLANGE","325 MM",null,"HANDWHEEL",null,"0-100 DEG C"]
["0688633","VALVE: TYPE: KNIFE GATE; VALVE SIZE: 450 MM; DESIGN RATING: 7 BAR; TEMPERATURE RATING: 50 DEG C; FACE TO FACE LENGTH: 143 MM; CONNECTION: FLANGE; OPERATED: HYDRAULIC ACTUATOR; BODY MATERIAL: CS; 16-HOLE EQUI-SPACED, OFF CRS ON A 585 PCD; 10-HOLES DRILL DIAMETER 26 THRU; 6-HOLES DRILL AND TAP M24 X 30 DEEP","PV ENGINEERING","KNIFE GATE","450 MM","CS","7 BAR",null,"FLANGE","143 MM","16-HOLE EQUI-SPACED, OFF CRS ON A 585 PCD","HYDRAULIC ACTUATOR",null,"50 DEG C"]
["0754499","VALVE, CHECK: TYPE: CHECK VALVE; VALVE SIZE: ¼ BSPT MALE DOWNSTREAM / 8L MALE UPSTREAM IN; DESIGN RATING: 500 BAR; TEMPERATURE RATING: -10 to +100 DEG C; CONNECTION: ¼ INCH BSPT MALE DOWNSTREAM / 8L MALE UPSTREAM; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 47.5 MM; OPERATED: PRESSURE; STYLE: HYDRAULIC; TRIM: STELLITED; APPLICATION: GREASE SYSTEM; SPECIFICATION: RHZ-R-ED",null,"CHECK; CHECK VALVE","¼ BSPT MALE DOWNSTREAM / 8L MALE UPSTREAM IN","STAINLESS STEEL","500 BAR","STELLITED","¼ INCH BSPT MALE DOWNSTREAM / 8L MALE UPSTREAM","47.5 MM",null,"PRESSURE","GREASE SYSTEM","-10 to +100 DEG C"]

{"sheet":"Gourikwa OCGT Power Station","index":11,"n_rows":74,"n_cols":14,"rows_kept":74}
["Material","Original Description","OEM / Manufacturer","Valve Type","Size","Body Material","Class / Rating","Trim / Internals","End Connection","Face-to-Face","Drilling / PCD","Operation","Medium / Service","Medium Temperature"]
["0233792","VALVE, SOLENOID: PIPE SIZE: DN15; STYLE: 2 WAY; POTENTIAL: 220 VDC; DESIGN RATING: 100 BAR; CONNECTION: FLANGE; BODY MATERIAL: GR 1.4404/1.4571; OPERATED: NO; ENCLOSURE RATING: IP65; MEDIUM: HEIZOL; CURRENT: 0.22 A; ORIFICE SIZE: DN 15; COIL: 220 V DC; MANUF P/N: FK15NO1E; SUPPL P/N: A2A50187268; REFERENCE NO: PB0000144283; 503443; 2.5 M3/HR; WITH 4 X 14 MM DIA HOLES DRILLED INTO FLANGE","Muller Coax","SOLENOID","DN15; DN 15","GR 1.4404/1.4571","100 BAR",null,"FLANGE",null,null,"NO","HEIZOL"]
["0233844","VALVE, CHECK: BODY MATERIAL: CI; SUPPL P/N: MBV30AA201; C5V08311B5; LIFTING OIL; KKS; FOR USE ON LIFTING OIL PUMP MBV BASE PIPING ON GT AUX SYSTEM","Parker","CHECK",null,"CI",{"$nulls":6},"LIFTING OIL PUMP MBV BASE PIPING ON GT AUX SYSTEM"]
["0233849","VALVE, BALL: VALVE SIZE: 1 IN; DESIGN RATING: 40 BAR; CONNECTION: BSP; BODY MATERIAL: STAINLESS STEEL; OPERATED: LEVER; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: PTFE; SUPPL P/N: MBV23AA412; REFERENCE NO: SLV3800141; MBV25AA401; WITH ATTACHMENT, KKS; FOR USE ON LUBE OIL FILTER ON MBV BASE PIPING ON GT AUX SYSTEM",null,"BALL","1 IN","STAINLESS STEEL","40 BAR","STAINLESS STEEL","BSP",null,null,"LEVER","LUBE OIL FILTER ON MBV BASE PIPING ON GT AUX SYSTEM"]
["0233850","VALVE: TYPE: ISOLATING; VALVE SIZE: NB 4; DESIGN RATING: 400 BAR; CONNECTION: BSP; OPERATED: HANDWHEEL; BODY MATERIAL: 1.046; STYLE: ISOLATE/VENT; REFERENCE NO: MBV31AA301; MBV31AA305; MBV21AA301; MBV23AA301; FOR USE ON GT AUX SYSTEMS",null,"ISOLATING","NB 4","1.046","400 BAR",null,"BSP",null,null,"HANDWHEEL","GT AUX SYSTEMS"]
["0233851","VALVE: TYPE: BALANCE; VALVE SIZE: 3/8 IN; DESIGN RATING: 16 BAR; TEMPERATURE RATING: 80-100 DEG C; CONNECTION: 3/8 IN-BSPP; OPERATED: KNOB; BODY MATERIAL: STL HARDENED BS 970; SPECIFICATION: 305000; SPECIAL FEATURES: HAND WHEEL; STL VERSION; MANUF P/N: 305000; REFERENCE NO: SLV3800141; MBV25AA252; FOR USE ON LUBE OIL FILTER ON MBV BASE PIPING ON GT AUX SYSTEM",null,"BALANCE","3/8 IN","STL HARDENED BS 970","16 BAR",null,"3/8 IN-BSPP",null,null,"KNOB","LUBE OIL FILTER ON MBV BASE PIPING ON GT AUX SYSTEM","80-100 DEG C"]
["0233857","VALVE, BUTTERFLY: TYPE: WAFER; VALVE SIZE: 150 MM; DESIGN RATING: PN16; TEMPERATURE RATING: -10 TO 80 DEG C; CONNECTION: FLANGE; BODY MATERIAL: STEEL; OPERATED: HANDLEVER; TRIM: STAINLESS STEEL; SOFTGOODS: RUBBER; REFERENCE NO: MBV21AA254; ECLS 71391; FOR USE ON MBV BASE PIPING ON GT AUX SYSTEM",null,"BUTTERFLY; WAFER","150 MM","STEEL","PN16","STAINLESS STEEL","FLANGE",null,null,"HANDLEVER","MBV BASE PIPING ON GT AUX SYSTEM","-10 TO 80 DEG C"]
["0233871","VALVE, RELIEF: BODY MATERIAL: CAST IRON; DESIGN RATING: 210 BAR; SUPPL P/N: MBA30AA191; R5V 08 593 32 A5 152 210; REFERENCE NO: SLV 3720522; PARKER; KKS: FOR LIFTING OIL PUMP ON GT AUX SYSTEM","Parker","RELIEF",null,"CAST IRON","210 BAR"]
["0233872","VALVE, RELIEF: BODY MATERIAL: CI; SUPPL P/N: R4V06 535 30 A5; MBV31AA151; REFERENCE NO: SLV3860114; PARKER, KKS; FOR CONTROL BLOCK LIFTING OIL ON MBV BASE PIPING ON GT AUX SYSTEM","Parker","RELIEF",null,"CI"]
["0233891","VALVE, BALL: VALVE SIZE: 1/4 IN; DESIGN RATING: 65; CONNECTION: THD; BODY MATERIAL: STAINLESS STEEL; OPERATED: LEVER; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: TEFLON; SUPPL P/N: MBV50AA503; KKS; USED ON MBV BASE PIPING ON GT AUX SYSTEMS",null,"BALL","1/4 IN","STAINLESS STEEL","65","STAINLESS STEEL","THD",null,null,"LEVER","MBV BASE PIPING ON GT AUX SYSTEMS"]
["0233892","VALVE, BALL: VALVE SIZE: 1/2 IN; DESIGN RATING: 65 BAR; CONNECTION: THD; BODY MATERIAL: STAINLESS STEEL; OPERATED: LEVER; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: TEFLON; SUPPL P/N: MBV21AA403; KKS; USED ON MBV BASE PIPING ON GT AUX SYSTEMS",null,"BALL","1/2 IN","STAINLESS STEEL","65 BAR","STAINLESS STEEL","THD",null,null,"LEVER","MBV BASE PIPING ON GT AUX SYSTEMS"]
["0233893","VALVE, BALL: VALVE SIZE: 3/4 IN; DESIGN RATING: 40; CONNECTION: THD; BODY MATERIAL: STAINLESS STEEL; OPERATED: LEVER; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: TEFLON; SUPPL P/N: MBV26AA401; KKS; USED ON MBV BASE PIPING ON GT AUX SYSTEMS",null,"BALL","3/4 IN","STAINLESS STEEL","40","STAINLESS STEEL","THD",null,null,"LEVER","MBV BASE PIPING ON GT AUX SYSTEMS"]
["0233895","VALVE, RELIEF: VALVE SIZE: 3/4 X 1/2 IN; SET PRESSURE: 10 BAR; CONNECTION: BSP; BODY MATERIAL: BRASS; TRIM: BRASS; OPERATED: PRESSURE; SUPPL P/N: MBV23AA191; KKS; USED ON GT AUX SYSTEMS",null,"RELIEF","3/4 X 1/2 IN","BRASS","10 BAR","BRASS","BSP",null,null,"PRESSURE","GT AUX SYSTEMS"]
["0233896","VALVE: TYPE: THROTTLE; OPERATED: KEY LOCK; BODY MATERIAL: STL; REFERENCE NO: MBV31AA285; USED ON CONTROL BLOCK ON MBV BASE PIPING ON GT AUX SYSTEMS",null,"THROTTLE",null,"STL",{"$nulls":5},"KEY LOCK","CONTROL BLOCK ON MBV BASE PIPING ON GT AUX SYSTEMS"]
["0233898","VALVE, BALL: VALVE SIZE: 2 IN; DESIGN RATING: 40 BAR; CONNECTION: THD; BODY MATERIAL: STAINLESS STEEL; OPERATED: LEVER; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: TEFLON; SUPPL P/N: MBV10AA401; KKS; USED ON MBV BASE PIPING ON GT AUX SYSTEMS",null,"BALL","2 IN","STAINLESS STEEL","40 BAR","STAINLESS STEEL","THD",null,null,"LEVER","MBV BASE PIPING ON GT AUX SYSTEMS"]
["0233901","VALVE, CHECK: TYPE: NON RETURN; VALVE SIZE: 150 MM; DESIGN RATING: 10-40 BAR; CONNECTION: FLANGE; STYLE: 1 WAY; TRIM: 1.4408; GRADE: 1.057; SUPPL P/N: MBV21AA201; KKS, USED ON MBV BASE PIPING ON GT AUX SYSTEMS",null,"CHECK; NON RETURN","150 MM",null,"10-40 BAR","1.4408","FLANGE",{"$nulls":3},"MBV BASE PIPING ON GT AUX SYSTEMS"]
["0235772","VALVE: TYPE: ISOLATING GAUGE; VALVE SIZE: NB 4; DESIGN RATING: PN400; CONNECTION: THD 1/2 IN; OPERATED: MANUAL; BODY MATERIAL: 1.4571; STYLE: 1 WAY; TRIM: GR 1.4571; SOFTGOODS: GR 1.4571; WITH ONE KNOB; USED ON GAS 1 AUX SYSTEM",null,"ISOLATING GAUGE","NB 4","1.4571","PN400","GR 1.4571","THD 1/2 IN",null,null,"MANUAL","GAS 1 AUX SYSTEM"]
["0235781","VALVE, CHECK: VALVE SIZE: 80; DESIGN RATING: PN16; BODY MATERIAL: BRZ; OPERATED: SPRING; STYLE: 1 WAY; TRIM: DISC SS; SOFTGOODS: STAINLESS STEEL; SUPPL P/N: RK71; NON RETURN; WITH SPIRAL CENTERING RING; USED ON GAS 1 AUX SYSTEM; TEMPERATURE RATING: 13 BAR AT 250 DEG CEL",null,"CHECK","80","BRZ","PN16","DISC SS",{"$nulls":3},"SPRING","GAS 1 AUX SYSTEM","13 BAR AT 250 DEG CEL"]
["0235783","VALVE, RELIEF: VALVE SIZE: 3/4 IN; TEMPERATURE RATING: 130 DEG C; CONNECTION: FEMALE THD; BODY MATERIAL: CRNIMO-STAHL; OPERATED: AIR; DESIGN RATING: PN16; PRESSURE RANGE: 0-16 BAR; REFERENCE NO: 7146002; MANKENBURG; USED ON GAS 1 AUX SYSTEM.","Mankenburg","RELIEF","3/4 IN","CRNIMO-STAHL","PN16; 0-16 BAR",null,"FEMALE THD",null,null,"AIR","GAS 1 AUX SYSTEM","130 DEG C"]
["0238889","VALVE: TYPE: GAGE ISOLATING; VALVE SIZE: 4 MM; DESIGN RATING: PN400; CONNECTION: 1/2 IN-BSP; OPERATED: MANUAL; BODY MATERIAL: CI; STYLE: 1 WAY; TRIM: CI; REFERENCE NO: 061462-9515.002; COMPLETE WITH BLEED DOWN SCREW; USED ON GAS 1 PLANT","Wika","GAGE ISOLATING","4 MM","CI","PN400","CI","1/2 IN-BSP",null,null,"MANUAL","GAS 1 PLANT"]
["0239052","VALVE, BALL: VALVE SIZE: 1/2 IN; DESIGN RATING: 16 BAR; CONNECTION: THD FEMALE; BODY MATERIAL: STAINLESS STEEL; OPERATED: WING GREEN; STYLE: 1 WAY; TRIM: TEFLON; FOR USE ON GAS 1 PLANT",null,"BALL","1/2 IN","STAINLESS STEEL","16 BAR","TEFLON","THD FEMALE",null,null,"WING GREEN","GAS 1 PLANT"]
["0239053","VALVE, RELIEF: VALVE SIZE: 1 IN; SET PRESSURE: 5.6 BAR; CONNECTION: THD; BODY MATERIAL: CI; OPERATED: PRESSURE; STYLE: 1 WAY; SUPPL P/N: 4593.2504; FOR USE ON GAS 1 PLANT",null,"RELIEF","1 IN","CI","5.6 BAR",null,"THD",null,null,"PRESSURE","GAS 1 PLANT"]
["0239054","VALVE, RELIEF: VALVE SIZE: 1 IN; SET PRESSURE: 6 BAR; CONNECTION: THD; BODY MATERIAL: CI; OPERATED: PRESSURE; STYLE: 1 WAY; SUPPL P/N: 4603.7863; TYPE SAFETY; TYPE LESER; FOR USE ON GAS 1 PLANT","SAFETY; LESER","RELIEF","1 IN","CI","6 BAR",null,"THD",null,null,"PRESSURE","GAS 1 PLANT"]
["0239649","VALVE, BALL: VALVE SIZE: 1/2 IN; DESIGN RATING: 16; TEMPERATURE RATING: -20 TO 130 DEG C; CONNECTION: THD 1/2 IN; BODY MATERIAL: BRS NICKEL PLTD; FACE TO FACE LENGTH: 50 MM; OPERATED: LEVER; STYLE: 1 WAY VALVE AND PLUG; APPLICATION: WATER; SUPPL P/N: 305220108",null,"BALL","1/2 IN","BRS NICKEL PLTD","16",null,"THD 1/2 IN","50 MM",null,"LEVER","WATER","-20 TO 130 DEG C"]
["0239669","VALVE, SOLENOID: PIPE SIZE: DN15; STYLE: 2/2 WAY; POTENTIAL: 24 VDC; DESIGN RATING: 0-40 BAR; CONNECTION: FLANGE; BODY MATERIAL: STAINLESS STEEL; OPERATED: SOLENOID; ENCLOSURE RATING: IP65; MEDIUM: DEMINIRALIZED WATER 70; POWER: 24 V X 1.6 A; CURRENT: 1.6 A; ORIFICE SIZE: DN 15; SOFTGOODS: SEAL VITON; APPLICATION: DEMIN WATER; SPECIFICATION: COAX VALVE; MANUF P/N: FK15NC; REFERENCE NO: 513465","Coax","SOLENOID","DN15; DN 15","STAINLESS STEEL","0-40 BAR",null,"FLANGE",null,null,"SOLENOID","DEMINIRALIZED WATER 70; DEMIN WATER"]
["0239684","VALVE, RELIEF: VALVE SIZE: 1 IN; SET PRESSURE: 10 BAR; CONNECTION: THD; BODY MATERIAL: BRASS; TRIM: BRASS; OPERATED: PRESSURE; DESIGN RATING: 25 BAR; PRESSURE RANGE: 0-25 BAR; SUPPL P/N: TUVSV 03-581 18",null,"RELIEF","1 IN","BRASS","25 BAR; 0-25 BAR; 10 BAR","BRASS","THD",null,null,"PRESSURE"]
["0239791","VALVE, RELIEF: VALVE SIZE: DN 32, 140 MM; SET PRESSURE: 22 BAR; CONNECTION: FLANGE, 140 MM; BODY MATERIAL: STAINLESS STEEL; TRIM: STAINLESS STEEL; FACE TO FACE LENGTH: 275 MM; OPERATED: SPRING; APPLICATION: TURBINE PURGE WATER OVERFLOW CONTROL; GRADE: 1.4408; DESIGN RATING: PN40; VALVE MADE OF CAST STEEL; SEAT,CONE,GUID CONE SPINDLE OF HIGH QUALITY STEEL; CENTRAL SPRING, DIN PN40; WILLEM SCHLEY HAMBURG - OVERFLOW VALVE MODEL T27","WILLEM SCHLEY HAMBURG - OVERFLOW VALVE; Willem Schley","RELIEF","DN 32, 140 MM","STAINLESS STEEL","PN40; 22 BAR","STAINLESS STEEL","FLANGE, 140 MM","275 MM",null,"SPRING","TURBINE PURGE WATER OVERFLOW CONTROL"]
["0239795","VALVE, CHECK: TYPE: NON RETURN; VALVE SIZE: 150 MM; DESIGN RATING: PN40; CONNECTION: FLANGE; BODY MATERIAL: STAINLESS STEEL; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SUPPL P/N: RK86A","Gestra","CHECK; NON RETURN","150 MM","STAINLESS STEEL","PN40","STAINLESS STEEL","FLANGE"]
["0250048","VALVE, CHECK: APPLICATION: CENTRIFUGES; MANUF P/N: 176289482; CAPACITY 2.8 L/MIN","Alva-Laval","CHECK",{"$nulls":8},"CENTRIFUGES"]
["0250049","VALVE, CHECK: APPLICATION: CENTRIFUGES; MANUF P/N: 176289486; OPERATED FLOW, CAPACITY 23 L/MIN","Alva-Laval","CHECK",{"$nulls":8},"CENTRIFUGES"]
["0250052","VALVE, SOLENOID: PIPE SIZE: 3/4 X 1 IN; STYLE: 4/2 WAY; POTENTIAL: 24 VDC; DESIGN RATING: 17 BAR; CONNECTION: NPT; BODY MATERIAL: BRASS; OPERATED: ELECTRONIC; ENCLOSURE RATING: IP65; MEDIUM: OIL/WATER; POWER: 11.6 W; CURRENT: 0.48 A; ORIFICE SIZE: 19 MM; COIL: SINGLE; APPLICATION: SSS CLUTCH; SPECIFICATION: SOLINOID VALVE; MANUF P/N: SC8344G076; REFERENCE NO: SC8344G076","Asco (Automatic Switch)","SOLENOID","3/4 X 1 IN; 19 MM","BRASS","17 BAR",null,"NPT",null,null,"ELECTRONIC","OIL/WATER; SSS CLUTCH"]
["0250052","VALVE, SOLENOID: PIPE SIZE: 3/4 X 1 IN; STYLE: 4/2 WAY; POTENTIAL: 24 VDC; DESIGN RATING: 17 BAR; CONNECTION: NPT; BODY MATERIAL: BRASS; OPERATED: ELECTRONIC; ENCLOSURE RATING: IP65; MEDIUM: OIL/WATER; POWER: 11.6 W; CURRENT: 0.48 A; ORIFICE SIZE: 19 MM; COIL: SINGLE; APPLICATION: SSS CLUTCH; SPECIFICATION: SOLINOID VALVE; MANUF P/N: SC8344G076; REFERENCE NO: SC8344G076",null,"SOLENOID","3/4 X 1 IN; 19 MM","BRASS","17 BAR",null,"NPT",null,null,"ELECTRONIC","OIL/WATER; SSS CLUTCH"]
["0257026","VALVE, BALL: VALVE SIZE: 40 MM; DESIGN RATING: 100; TEMPERATURE RATING: -10 TO 200 DEG C; CONNECTION: FLANGE; BODY MATERIAL: STEEL; FACE TO FACE LENGTH: 250; OPERATED: ACTUATOR ELECTRIC; GRADE: I54; TYPE: PREMIX","Argus","BALL; PREMIX","40 MM","STEEL","100",null,"FLANGE","250",null,"ACTUATOR ELECTRIC",null,"-10 TO 200 DEG C"]
["0553121","VALVE, SOLENOID: PIPE SIZE: 1/2 IN; STYLE: (2) PIPE CONNECTIONS; (1) SOLENOID; POTENTIAL: 220 VDC; DESIGN RATING: 0-100 BAR; CONNECTION: TERMINAL; BODY MATERIAL: GS/BRS; OPERATED: COIL; ENCLOSURE RATING: IP65; MEDIUM: DIESEL; POWER: 40 W; CURRENT: 0.17 A DC; ORIFICE SIZE: G 1/2 IN; COIL: 220 VOLT DC INSULATION CLASS - H; SOFTGOODS: VITON SEALS; APPLICATION: DIFFUSION/PREMIX FUEL LINES V9214 GAS TURBINES; SPECIFICATION: MK15NC2E; CLASSIFICATION: E X NA11 T3; MANUF P/N: MK15NC2E; 523181; TERMINAL 130 X M15 X 1.5 MM","Muller Coax","SOLENOID","1/2 IN; G 1/2 IN","GS/BRS","0-100 BAR",null,"TERMINAL",null,null,"COIL","DIESEL; DIFFUSION/PREMIX FUEL LINES V9214 GAS TURBINES"]
["0553122","VALVE: TYPE: SOLENOID COAXIAL; VALVE SIZE: G10/0; DESIGN RATING: 40 BAR; TEMPERATURE RATING: -40 TO 100 DEG C; CONNECTION: 1/2 IN; OPERATED: ELECTRIC COIL 220VAC; BODY MATERIAL: BRASS; SPECIFICATION: VALVE; SOFTGOODS: VITON; SPECIAL FEATURES: VITON SEAL; MANUF P/N: MK25DRN01E; 510038","Coax","SOLENOID COAXIAL","G10/0","BRASS","40 BAR",null,"1/2 IN",null,null,"ELECTRIC COIL 220VAC",null,"-40 TO 100 DEG C"]
["0553123","VALVE: TYPE: SOLONOID COAXIAL; VALVE SIZE: PN40; DESIGN RATING: 0-40 BAR; TEMPERATURE RATING: -40 TO 100 DEG C; CONNECTION: FLANGE PN40; OPERATED: ELECTRIC COIL 230VAC; BODY MATERIAL: BRASS; SPECIFICATION: VALVE; SOFTGOODS: VITON; SPECIAL FEATURES: VITON SEALS; MANUF P/N: 515259; FK25NC1E","Coax","SOLONOID COAXIAL","PN40","BRASS","0-40 BAR",null,"FLANGE PN40",null,null,"ELECTRIC COIL 230VAC",null,"-40 TO 100 DEG C"]
["0553124","VALVE: TYPE: SOLONOID COAXIAL; VALVE SIZE: PN40; DESIGN RATING: 0-40 BAR; TEMPERATURE RATING: -40 TO 100 DEG C; CONNECTION: FLANGE; OPERATED: ELECTRIC COIL 240VAC; BODY MATERIAL: BRASS; SPECIFICATION: VALVE; SOFTGOODS: VITON; SPECIAL FEATURES: VITON SEALS; MANUF P/N: 527506; FK25NC","Coax","SOLONOID COAXIAL","PN40","BRASS","0-40 BAR",null,"FLANGE",null,null,"ELECTRIC COIL 240VAC",null,"-40 TO 100 DEG C"]
["0553125","VALVE: TYPE: SOLONOID COAXIAL; VALVE SIZE: NB8 MM; DESIGN RATING: 0-150 BAR; TEMPERATURE RATING: 55 DEG C; CONNECTION: 3/8 IN THREAD; OPERATED: ELECTRIC COIL 220VDC; BODY MATERIAL: BRASS; SPECIFICATION: VALVE; SOFTGOODS: VITON; MANUF P/N: 503507; ECD-H10NO2E","Coax","SOLONOID COAXIAL","NB8 MM","BRASS","0-150 BAR",null,"3/8 IN THREAD",null,null,"ELECTRIC COIL 220VDC",null,"55 DEG C"]
["0553126","VALVE: TYPE: COAXIAL SOLENOID; VALVE SIZE: G11/4; 38 MM; DESIGN RATING: 0-100 BAR; TEMPERATURE RATING: -40 TO 100 DEG C; CONNECTION: 1-1/4 IN THREAD; OPERATED: ELECTRIC COIL 220VDC; BODY MATERIAL: BRASS; SOFTGOODS: VITON; MANUF P/N: 500479; MK25NC1E","Coax","COAXIAL SOLENOID","G11/4","BRASS","0-100 BAR",null,"1-1/4 IN THREAD",null,null,"ELECTRIC COIL 220VDC",null,"-40 TO 100 DEG C"]
["0553127","VALVE: TYPE: SOLENOID COAXIAL; VALVE SIZE: PN100; DESIGN RATING: 0-100 BAR; TEMPERATURE RATING: -40 TO 100 DEG C; FACE TO FACE LENGTH: 241 MM; CONNECTION: THREAD/FLANGE; OPERATED: ELECTRIC COIL 220VDC; BODY MATERIAL: BRASS; SPECIFICATION: VALVE; SOFTGOODS: VITON; SPECIAL FEATURES: VITON SEALS; MANUF P/N: 527372; FKI5NC1E","Coax","SOLENOID COAXIAL","PN100","BRASS","0-100 BAR",null,"THREAD/FLANGE","241 MM",null,"ELECTRIC COIL 220VDC",null,"-40 TO 100 DEG C"]
["0553128","VALVE: TYPE: SOLONOID COAXIAL; VALVE SIZE: G1/2; DESIGN RATING: 0-100 BAR; TEMPERATURE RATING: -40 TO 100 DEG C; CONNECTION: THREAD/FLANGE; OPERATED: ELECTRIC COIL 230VAC; BODY MATERIAL: BRASS; SPECIFICATION: VALVE; SOFTGOODS: VITON; MANUF P/N: MK15NC1E; 520496","Coax","SOLONOID COAXIAL","G1/2","BRASS","0-100 BAR",null,"THREAD/FLANGE",null,null,"ELECTRIC COIL 230VAC",null,"-40 TO 100 DEG C"]
["0553129","VALVE: TYPE: INLINE SOLENOID; VALVE SIZE: G1/2 IN-BSPP; DESIGN RATING: 0-40 BAR; TEMPERATURE RATING: -40 TO 100 DEG C; FACE TO FACE LENGTH: 184 MM; CONNECTION: THD; OPERATED: ELECTRIC COIL 220VDC; BODY MATERIAL: GS/BRS; STYLE: 2/2 WAY DIRECT ACTING; TRIM: BODY MATERIAL BRASS/GALVANISED STEEL; SPECIFICATION: VALVE; SOFTGOODS: VITON; SPECIAL FEATURES: 2 X INDUCTIVE PROXIMITY SWITCHES/SAME DIRECTION SWITCHING; MANUF P/N: 503506; MK15NC2E","Muller Coax","INLINE SOLENOID","G1/2 IN-BSPP","GS/BRS","0-40 BAR","BODY MATERIAL BRASS/GALVANISED STEEL","THD","184 MM",null,"ELECTRIC COIL 220VDC",null,"-40 TO 100 DEG C"]
["0585702","VALVE, SOLENOID: PIPE SIZE: G3/8 IN; STYLE: 2/2 WAY; POTENTIAL: 220 VDC; DESIGN RATING: 0-150 BAR; CONNECTION: THD; BODY MATERIAL: BRASS; OPERATED: SOLENOID; ENCLOSURE RATING: IP65; MEDIUM: FUEL/OIL; ORIFICE SIZE: 10 MM; SOFTGOODS: VITON SEALS; APPLICATION: FUEL/OIL; SPECIFICATION: 516348; CLASSIFICATION: ZONE 2; MANUF P/N: ECD-H10NO2E; 2 LIMIT SWITCHES, 55 DEG; HIGH PRESSURE","Muller Coax","SOLENOID","G3/8 IN; 10 MM","BRASS","0-150 BAR",null,"THD",null,null,"SOLENOID","FUEL/OIL"]
["0588761","VALVE, BUTTERFLY: TYPE: SWIVEL; VALVE SIZE: 400 MM; DESIGN RATING: 6 BAR; TEMPERATURE RATING: 270 DEG C; CONNECTION: FLANGE; BODY MATERIAL: STEEL WELDMENT; FACE TO FACE LENGTH: 310 MM; OPERATED: ACTUATOR PNEUMATIC; TRIM: FLEXIBLE PRESS FORMED; SOFTGOODS: PTFE COMPOUND; APPLICATION: TURBINE COMPRESSOR; GRADE: PN10; DIN 2632; DRAWING NO: 1.5055B REV 0; INCLUDING ACTUATOR: ACTUATOR POSITION SLV 3540043 (TOP)","Friedrich Krombach","BUTTERFLY; SWIVEL","400 MM","STEEL WELDMENT","6 BAR","FLEXIBLE PRESS FORMED","FLANGE","310 MM",null,"ACTUATOR PNEUMATIC; ACTUATOR POSITION SLV 3540043 (TOP)","TURBINE COMPRESSOR","270 DEG C"]
["0593549","VALVE, BUTTERFLY: TYPE: SWIVEL; VALVE SIZE: 400 MM; DESIGN RATING: 6 BAR; TEMPERATURE RATING: 270 DEG C; CONNECTION: FLANGE; BODY MATERIAL: STEEL WELDMENT; FACE TO FACE LENGTH: 310 MM; OPERATED: ACTUATOR PNEUMATIC; TRIM: FLEXIBLE PRESS FORMED; SOFTGOODS: PTFE COMPOUND; APPLICATION: TURBINE COMPRESSOR; GRADE: PN10; DIN 2632; DRAWING NO: 1.5055B REV 0; INCLUDING ACTUATOR; ACTUATOR POSITION SLV 3540041 L/H","Friedrich Krombach","BUTTERFLY; SWIVEL","400 MM","STEEL WELDMENT","6 BAR","FLEXIBLE PRESS FORMED","FLANGE","310 MM",null,"ACTUATOR PNEUMATIC","TURBINE COMPRESSOR","270 DEG C"]
["0593550","VALVE, BUTTERFLY: TYPE: SWIVEL; VALVE SIZE: 400 MM; DESIGN RATING: 6 BAR; TEMPERATURE RATING: 270 DEG C; CONNECTION: FLANGE; BODY MATERIAL: STEEL WELDMENT; FACE TO FACE LENGTH: 310 MM; OPERATED: ACTUATOR PNEUMATIC; TRIM: FLEXIBLE PRESS FORMED; SOFTGOODS: PTFE COMPOUND; APPLICATION: TURBINE COMPRESSOR; GRADE: PN10; DIN 2632; DRAWING NO: 1.5055B REV 0; INCLUDING ACTUATOR; ACTUATOR POSITION SLV 3540042 R/H","Friedrich Krombach","BUTTERFLY; SWIVEL","400 MM","STEEL WELDMENT","6 BAR","FLEXIBLE PRESS FORMED","FLANGE","310 MM",null,"ACTUATOR PNEUMATIC","TURBINE COMPRESSOR","270 DEG C"]
["0593794","KIT: TYPE: SEAL; APPLICATION: CHANGE OVER VALVE HDD 91; COMPRISING: O-RINGS; SUPPORT RINGS; MANUF P/N: 318517; ALL O RINGS FROM VITON MATERIAL - HDD91 CHANGE OVER VALVE",null,"SEAL",{"$nulls":8},"CHANGE OVER VALVE HDD 91"]
["0593797","KIT: TYPE: SEAL; APPLICATION: CHANGE OVER VALVE HDD 170; COMPRISING: O-RINGS; SUPPORT RINGS; MANUF P/N: 308333; ALL O RINGS FROM VITON MATERIAL - HDD 170 CHANGE OVER VALVE",null,"SEAL",{"$nulls":8},"CHANGE OVER VALVE HDD 170"]
["0607158","VALVE, BALL: VALVE SIZE: 40 MM; DESIGN RATING: 100 BAR; TEMPERATURE RATING: -10 TO 200 DEG C; CONNECTION: FLANGE; BODY MATERIAL: STEEL; FACE TO FACE LENGTH: 850 MM; OPERATED: ACTUATOR/ELECTRICAL; GRADE: I54; TYPE: FUEL DIFFUSION; MANUF P/N: 5100046637-100; 6211-0100-670289/G84/G82G; VALVE AND ACTUATOR ASSEMBLY","Argus","BALL; FUEL DIFFUSION","40 MM","STEEL","100 BAR",null,"FLANGE","850 MM",null,"ACTUATOR/ELECTRICAL",null,"-10 TO 200 DEG C"]
["0612657","VALVE, BALL: VALVE SIZE: DN 40; DESIGN RATING: PN100; TEMPERATURE RATING: -10 TO 200 DEG C; CONNECTION: FLANGE; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 300 MM; OPERATED: ELECTRICAL MOTOR; STYLE: 3 WAY; TYPE: PREMIX; SUPPL P/N: 6211-0100-670852MOD/-G85GH...M; VALVE AND ACTUATOR ASSEMBLY; ARGUS E25 ELECTRIC ACTUATOR, VALVE AND ELECTRIC ACTUATOR ASSEMBLY A2A50296201/ PB0000279980","Argus","BALL; PREMIX","DN 40","STAINLESS STEEL","PN100",null,"FLANGE","300 MM",null,"ELECTRICAL MOTOR",null,"-10 TO 200 DEG C"]
["0613732","VALVE: TYPE: SOL; VALVE SIZE: 15 MM; TEMPERATURE RATING: MAX 160 DEG C; FACE TO FACE LENGTH: 130 MM; CONNECTION: FLANGE; OPERATED: ELECTRICAL; BODY MATERIAL: STAINLESS STEEL; OEM P/N: 12-EVF 5R U.XN.P.09.29; A2A50268346; SUPPL P/N: 799.010.010.0421; 220 VDC","Argus","SOL","15 MM","STAINLESS STEEL",null,null,"FLANGE","130 MM",null,"ELECTRICAL",null,"MAX 160 DEG C"]
["0613733","VALVE: TYPE: SOL; VALVE SIZE: 15 MM; TEMPERATURE RATING: MAX 160 DEG C; FACE TO FACE LENGTH: 130 MM; CONNECTION: FLANGE; OPERATED: ELECTRICAL; BODY MATERIAL: STAINLESS STEEL; OEM P/N: 12-EVDF 3R XN.W.U.P.09.29; SUPPL P/N: 799.010.010.0422; A2A50268347; 220 VDC","Uni Gerate","SOL","15 MM","STAINLESS STEEL",null,null,"FLANGE","130 MM",null,"ELECTRICAL",null,"MAX 160 DEG C"]
["0613741","VALVE: TYPE: NON RETURN,WAFER; VALVE SIZE: 54 MM; DESIGN RATING: 160 BAR; TEMPERATURE RATING: 300 DEG C; FACE TO FACE LENGTH: 25 MM; CONNECTION: COUPLING; OPERATED: PNEUMATIC; BODY MATERIAL: STAINLESS STEEL; STYLE: WAFER; TRIM: DISC SS; OEM P/N: A2A50005975; SUPPL P/N: 700.050.010.1028",null,"NON RETURN,WAFER","54 MM","STAINLESS STEEL","160 BAR","DISC SS","COUPLING","25 MM",null,"PNEUMATIC",null,"300 DEG C"]
["0621637","SET: TYPE: STOP VALVE; OEM P/N: A2A50314606; SUPPL P/N: PG0031759200",null,"STOP VALVE"]
["0622490","VALVE, SOLENOID: PIPE SIZE: DN25; STYLE: 1/2; POTENTIAL: 220 V; DESIGN RATING: PN40; CONNECTION: FLANGE; BODY MATERIAL: STEEL; OPERATED: ELECTRIC; ENCLOSURE RATING: IP65; MEDIUM: BUTANE/NATURAL GAS/PROPANE; CURRENT: 0.33 A; OEM P/N: A2A50272850; SUPPL P/N: PB0000267703",null,"SOLENOID","DN25","STEEL","PN40",null,"FLANGE",null,null,"ELECTRIC","BUTANE/NATURAL GAS/PROPANE"]
["0622492","VALVE, SOLENOID: PIPE SIZE: DN25; STYLE: 2/2; POTENTIAL: 230 V; DESIGN RATING: PN40; CONNECTION: FLANGE; BODY MATERIAL: STEEL; OPERATED: ELECTRIC; ENCLOSURE RATING: IP65; MEDIUM: BUTANE/NATURAL GAS/PROPANE; POWER: 160 W; CURRENT: 0.33 A; SPECIFICATION: DIN 3394-1; OEM P/N: 40-EVSADU 10NH-4 P.XN.09.20.32; SUPPL P/N: PB0000282466; A2A50296211","Uni Gerate","SOLENOID","DN25","STEEL","PN40",null,"FLANGE",null,null,"ELECTRIC","BUTANE/NATURAL GAS/PROPANE"]
["0622742","VALVE: TYPE: FUEL OIL TRANSFER; VALVE SIZE: G1/2 IN; TEMPERATURE RATING: MAX 140 DEG C; CONNECTION: FLANGE, FITTING; OPERATED: AUTOMATIC; BODY MATERIAL: STEEL; OEM P/N: A2A50323268; SUPPL P/N: PG0032860600",null,"FUEL OIL TRANSFER","G1/2 IN","STEEL",null,null,"FLANGE, FITTING",null,null,"AUTOMATIC",null,"MAX 140 DEG C"]
["0622743","VALVE: TYPE: FUEL OIL PREMIX; VALVE SIZE: G1/2 IN; DESIGN RATING: PN100; TEMPERATURE RATING: MAX 160 DEG C; CONNECTION: FLANGE, FITTING; OPERATED: AUTOMATIC; BODY MATERIAL: STEEL; OEM P/N: A2A50328041; SUPPL P/N: PG0032863600",null,"FUEL OIL PREMIX","G1/2 IN","STEEL","PN100",null,"FLANGE, FITTING",null,null,"AUTOMATIC",null,"MAX 160 DEG C"]
["0626656","VALVE, CHECK: TYPE: HYDRAULIC; VALVE SIZE: G1/2 IN; DESIGN RATING: MAX 350 BAR; TEMPERATURE RATING: -30 TO 80 DEG C; CONNECTION: G1/2 IN-BSPP; BODY MATERIAL: STEEL; FACE TO FACE LENGTH: 16 MM; OPERATED: PNEUMATIC; OEM P/N: PG0031832800; SUPPL P/N: A2A50315038",null,"CHECK; HYDRAULIC","G1/2 IN","STEEL","MAX 350 BAR",null,"G1/2 IN-BSPP","16 MM",null,"PNEUMATIC",null,"-30 TO 80 DEG C"]
["0643634","VALVE: TYPE: CONTROL; VALVE SIZE: 6 IN; DESIGN RATING: 21 BAR; TEMPERATURE RATING: 65 DEG C; FACE TO FACE LENGTH: 235 MM; CONNECTION: WAFER; OPERATED: PILOT; BODY MATERIAL: CS; SPECIFICATION: 799-D; REFERENCE NO: 139163","INBAL","CONTROL","6 IN","CS","21 BAR",null,"WAFER","235 MM",null,"PILOT",null,"65 DEG C"]
["0644167","VALVE: TYPE: STOP; VALVE SIZE: DN 50; DESIGN RATING: 16 BAR; TEMPERATURE RATING: 120 DEG C; FACE TO FACE LENGTH: 150 MM; CONNECTION: FLANGE; OPERATED: MANUAL; BODY MATERIAL: CAST IRON; GRADE: EN-JL1040; SPECIFICATION: ARI 12072; .",null,"STOP","DN 50","CAST IRON","16 BAR",null,"FLANGE","150 MM",null,"MANUAL",null,"120 DEG C"]
["0644168","VALVE: TYPE: STOP; VALVE SIZE: DN 40; DESIGN RATING: 16 BAR; TEMPERATURE RATING: 120 DEG C; FACE TO FACE LENGTH: 140 MM; CONNECTION: FLANGE 150 MM; OPERATED: MANUAL; BODY MATERIAL: CAST IRON; GRADE: EN-JL1040; SPECIFICATION: ARI 12072",null,"STOP","DN 40","CAST IRON","16 BAR",null,"FLANGE 150 MM","140 MM",null,"MANUAL",null,"120 DEG C"]
["0644441","VALVE: TYPE: CONTROL; VALVE SIZE: 2 IN; DESIGN RATING: 21 BAR; TEMPERATURE RATING: 65 DEG C; FACE TO FACE LENGTH: 190 MM; CONNECTION: FLANGE; OPERATED: PILOT; BODY MATERIAL: CS; SPECIFICATION: 711-D","INBAL","CONTROL","2 IN","CS","21 BAR",null,"FLANGE","190 MM",null,"PILOT",null,"65 DEG C"]
["0644442","VALVE: TYPE: CONTROL; VALVE SIZE: 3 IN; DESIGN RATING: 21 BAR; TEMPERATURE RATING: 65 DEG C; FACE TO FACE LENGTH: 155 MM; CONNECTION: WAFER; OPERATED: PILOT; BODY MATERIAL: CARBON STL; SPECIFICATION: 799-D","INBAL","CONTROL","3 IN","CARBON STL","21 BAR",null,"WAFER","155 MM",null,"PILOT",null,"65 DEG C"]
["0644443","VALVE: TYPE: CONTROL; VALVE SIZE: 4 IN; DESIGN RATING: 21 BAR; TEMPERATURE RATING: 65 DEG C; FACE TO FACE LENGTH: 187 MM; CONNECTION: WAFER; OPERATED: PILOT; BODY MATERIAL: CARBON STL; SPECIFICATION: 799-D","INBAL","CONTROL","4 IN","CARBON STL","21 BAR",null,"WAFER","187 MM",null,"PILOT",null,"65 DEG C"]
["0647831","VALVE, BALL: VALVE SIZE: 1 IN; DESIGN RATING: 69 BAR; TEMPERATURE RATING: 50 DEG C; CONNECTION: BSP THREADED ENDS; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 88 MM; OPERATED: MANUAL; SOFTGOODS: PTFE; PORT TYPE: FULL BORE; GRADE: ASTM A351 GR CF8M; 2 PIECE SERIES 20",null,"BALL; FULL BORE","1 IN","STAINLESS STEEL","69 BAR",null,"BSP THREADED ENDS","88 MM",null,"MANUAL",null,"50 DEG C"]
["0647832","VALVE, BALL: VALVE SIZE: 1/2 IN; DESIGN RATING: 69 BAR; TEMPERATURE RATING: 50 DEG C; CONNECTION: BSP THREADED ENDS; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 65 MM; OPERATED: MANUAL; SOFTGOODS: PTFE; PORT TYPE: FULL BORE; GRADE: ASTM A351 GR CF8M; 2 PIECE SERIES 20",null,"BALL; FULL BORE","1/2 IN","STAINLESS STEEL","69 BAR",null,"BSP THREADED ENDS","65 MM",null,"MANUAL",null,"50 DEG C"]
["0647833","VALVE, BALL: VALVE SIZE: 3/4 IN; DESIGN RATING: 69; TEMPERATURE RATING: 50 DEG C; CONNECTION: BSP THREADED ENDS; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 74 MM; OPERATED: MANUAL; SOFTGOODS: PTFE; PORT TYPE: FULL BORE; GRADE: ASTM A351 GR CF8M; 2 PIECE SERIES 20",null,"BALL; FULL BORE","3/4 IN","STAINLESS STEEL","69",null,"BSP THREADED ENDS","74 MM",null,"MANUAL",null,"50 DEG C"]
["0650143","VALVE, SOLENOID: PIPE SIZE: 3/4 IN; STYLE: 9 X CONNECTIONS; 3 X SOLENOID; POTENTIAL: 24 VDC; DESIGN RATING: 3 BAR; CONNECTION: BSP; BODY MATERIAL: BRASS; OPERATED: DIRECT SOLENOID; ENCLOSURE RATING: IP67; MEDIUM: WATER; POWER: 11.2 W; ORIFICE SIZE: 19 MM; COIL: DC; APPLICATION: CENTRIFUGE SEALING WATER; CLASSIFICATION: ZONE 2; SUPPL P/N: 176346680","Alva-Laval","SOLENOID","3/4 IN; 19 MM","BRASS","3 BAR",null,"BSP",null,null,"DIRECT SOLENOID","WATER; CENTRIFUGE SEALING WATER"]
["0650143","VALVE, SOLENOID: PIPE SIZE: DN15; STYLE: BLOCK; POTENTIAL: 24 VDC; DESIGN RATING: 0.2-16 BAR; CONNECTION: PLUG; BODY MATERIAL: BRASS; OPERATED: DC V; ENCLOSURE RATING: IP65; MEDIUM: AIR/WATER; POWER: 11 W; CURRENT: 0.46 A; ORIFICE SIZE: 13 MM; SOFTGOODS: SEAL NBR; APPLICATION: GAS TURBINE FIRE SYSTEM; SPECIFICATION: ISO; MANUF P/N: 840131","Burkert","SOLENOID","DN15; 13 MM","BRASS","0.2-16 BAR",null,"PLUG",null,null,"DC V","AIR/WATER; GAS TURBINE FIRE SYSTEM"]
["0671894","VALVE: TYPE: CHANGE OVER; VALVE SIZE: 1-1/2 IN; DESIGN RATING: 40-100 BAR; TEMPERATURE RATING: -10 TO 425 DEG C; FACE TO FACE LENGTH: 265 MM; CONNECTION: DN 40; OPERATED: HAND; BODY MATERIAL: GP 240GM + N 1.0619; STYLE: CHANGE OVER VALVE; TRIM: CR 1,4021; GRADE: CARBON STEEL; SOFTGOODS: GRAPHITE/1,4571; SPECIAL FEATURES: CHANGE OVER VALVE,3 PORTS FLANGE; PN - 300 LBS","Leser","3 PORTS FLANGE; CHANGE OVER","1-1/2 IN","GP 240GM + N 1.0619","40-100 BAR","CR 1,4021","DN 40","265 MM",null,"HAND",null,"-10 TO 425 DEG C"]
["0708469","VALVE: TYPE: DELUGE; VALVE SIZE: 3 IN; DESIGN RATING: 21 BAR; TEMPERATURE RATING: 65 DEG C; CONNECTION: WAFER; OPERATED: ACTUATOR HYDRAULIC; BODY MATERIAL: FORGED STEEL SAE1021; INBAL MODEL 799DG-04-A01 HYDRAULIC DELGE VALVE- WAGER PATTERN ENDS RATED TO 21 TO OPEN WHEN PRESSURE IS LOST IN THE LINE, LATCH IN OPEN POSITION, LOCAL RESET COMPLETE WITH ALL NECESSARY TRIM VALVE ENDS AND WATER FLOW TEST & DRAIN ENDS DUCTILE (ASTM A53665-45-12), SLEEVE SMR5 ELATOMER REINFORCED WITH POLYESTER AND KEVLAR, CONTROL TRIM BRASS NICKEL CHROME PLATED STAINLESS STEEL AND GALVANISED STEEL","INBAL","DELUGE","3 IN","FORGED STEEL SAE1021","21 BAR",null,"WAFER",null,null,"ACTUATOR HYDRAULIC",null,"65 DEG C"]
["0708473","VALVE: TYPE: DELUGE; VALVE SIZE: 4 IN; DESIGN RATING: 21 BAR; TEMPERATURE RATING: 65 DEG C; CONNECTION: WAFER; OPERATED: ACTUATOR HYDRAULIC; BODY MATERIAL: FORGED STEEL SAE1021; INBAL MODEL 799DG-04-A01 HYDRAULIC DELGE VALVE- WAGER PATTERN ENDS RATED TO 21 TO OPEN WHEN PRESSURE IS LOST IN THE LINE, LATCH IN OPEN POSITION, LOCAL RESET COMPLETE WITH ALL NECESSARY TRIM VALVE ENDS AND WATER FLOW TEST & DRAIN ENDS DUCTILE (ASTM A53665-45-12), SLEEVE SMR5 ELATOMER REINFORCED WITH POLYESTER AND KEVLAR, CONTROL TRIM BRASS NICKEL CHROME PLATED STAINLESS STEEL AND GALVANISED STEEL","INBAL","DELUGE","4 IN","FORGED STEEL SAE1021","21 BAR",null,"WAFER",null,null,"ACTUATOR HYDRAULIC",null,"65 DEG C"]
["0758582","VALVE: TYPE: NRV; VALVE SIZE: 3/8 IN; DESIGN RATING: 700 BAR; TEMPERATURE RATING: 0 to 80 DEG; FACE TO FACE LENGTH: 11.7 MM; CONNECTION: THREAD 1/4 INCH BSP; OPERATED: BALL, SPRING; BODY MATERIAL: STAINLESS STEEL; STYLE: 1 WAY; SPECIFICATION: HAWE HYDRAULICS RB2 NRV SIZE: 3/8” BSPP; SOFTGOODS: 0-RINGS, SPRINGS; SPECIAL FEATURES: HAWE HYDRAULICS RB2 NRV SIZE: 3/8” BSPP","Hawe","NRV","3/8 IN","STAINLESS STEEL","700 BAR",null,"THREAD 1/4 INCH BSP","11.7 MM",null,"BALL, SPRING",null,"0 to 80 DEG"]

{"sheet":"Ingula Pumped Storage Scheme","index":12,"n_rows":162,"n_cols":14,"rows_kept":162}
["Material","Original Description","OEM / Manufacturer","Valve Type","Size","Body Material","Class / Rating","Trim / Internals","End Connection","Face-to-Face","Drilling / PCD","Operation","Medium / Service","Medium Temperature"]
["0041833","VALVE: TYPE: COMPRESSOR; VALVE SIZE: 175 MM; OPERATED: PRESSURE; BODY MATERIAL: STL; TRIM: DISC SS; 2ND STAGE CONCENTRIC","SAUER COMPRESSOR","COMPRESSOR","175 MM","STL","27bar","DISC SS","N/A","N/A","N/A","PRESSURE","AIR","50C"]
["0062540","VALVE, SOLENOID: POTENTIAL: 220 V; SUPPL P/N: S2155",null,"SOLENOID"]
["0063385","SEAT: TYPE: DISC SAFETY VALVE; DIMENSIONS: SQ 0.514 IN; MATERIAL: 1.4122 DIN X 35CRMO17; SUPPL P/N: 018109610; 601267620; MODEL NO: VSE2.40.25.A.50.I.22.123; USED ON SEMPELL; POSITION CODE RL01S010, RL02S009, RL03S008","Sempell","DISC SAFETY VALVE","SQ 0,51410 IN","1.4122 DIN X 35CRMO17","P/N: 018109610; 601267620","SEAT","NO END CONNECTION","N/A","N/A","PASSIVE SEALING","SEMPELL","400-450°C"]
["0065928","BALL VLV:16 MM;STL","PISTER","Ball","16MM","STAINLESS STEEL","PN400","BALL, SEATS, STEM,SEALS","MALE CONNECTION","COMPACT, NON STANDARD DIMENSION","N/A","MANUAL","OIL","180°C"]
["0072645","VALVE: TYPE: HYDRAULIC; VALVE SIZE: 3/4 IN","PISTER/UFIXED/HYDEC","HYDRAULIC","3/4 IN","STAINLESS STEEL","315 – 500 bar ","STEEL","THREADED","N/A","N/A","MANUAL","OIL","0-80°C "]
["0619974","VALVE, RELIEF: VALVE SIZE: 1/2 IN; SET PRESSURE: 1.5 MPA; TEMPERATURE RATING: 120 DEG C; CONNECTION: BSP SCREW; BODY MATERIAL: STEEL; TRIM: STEEL; FACE TO FACE LENGTH: T-TYPE; OPERATED: PRESSURE; APPLICATION: PRESSURE REDUCER; DESIGN RATING: 1.5 MPA; PRESSURE RANGE: 1.3-1.5 MPA; REFERENCE NO: ESV-903M","LESER","RELIEF","1/2 IN","STEEL","1.5 MPA; 1.3-1.5 MPA","STEEL","BSP SCREW","T-TYPE","N/A","PRESSURE","PRESSURE REDUCER","120 DEG C"]
["0619983","VALVE, BALL: VALVE SIZE: 50 MM; DESIGN RATING: 10 KPA; TEMPERATURE RATING: JIS10K; CONNECTION: FLANGED; BODY MATERIAL: SCPH2/304; FACE TO FACE LENGTH: 175 MM; OPERATED: LEVER; STYLE: DIRECTIONAL; TRIM: STL; SOFTGOODS: PTFE; APPLICATION: UPPER OIL COOLER; TYPE: ISOLATING","PISTER,VALVES FOR AFRICA","BALL; ISOLATING","50 MM","SCPH2/304","10 KPA","STL","FLANGED","175 MM","N/A","LEVER","UPPER OIL COOLER","JIS10K"]
["0620183","VALVE, GLOBE: VALVE SIZE: 1/2 IN; DESIGN PRESSURE: 2.0 MPA; DESIGN TEMPERATURE: <100 DEG C; FACE TO FACE LENGTH: 150 MM; OPERATED: HANDWHEEL; CONNECTION: FLANGED; BODY MATERIAL: F304; TRIM: SS GR 304/STL; GRADE: ASTM A182 F304; SOFTGOODS: NEOPRENE; STEM DESIGN: RISING SPINDLE; STYLE: DIRECTIONAL; APPLICATION: DRAIN AIR/OIL COOLER; SPECIFICATION: ISO9001; TYPE: SHUT OFF; DESIGN RATING: JIS 20K; S AND S VALVE","S&S VALVE (SAVE BRAND), ","GLOBE; SHUT OFF","1/2 IN","F304","JIS 20K; 2.0 MPA","SS GR 304/STL; RISING SPINDLE","FLANGED","150 MM","N/A","HANDWHEEL","DRAIN AIR/OIL COOLER","<100 DEG C"]
["0620391","VALVE, GATE: VALVE SIZE: 250 MM; TYPE: ISOLATING; DESIGN PRESSURE: 2-2.8 MPA; DESIGN TEMPERATURE: 220-350 DEG C; CONNECTION: FLANGE; FACE TO FACE LENGTH: 455 MM; BODY MATERIAL: STAINLESS STEEL; TRIM: HF; OPERATED: ACTUATOR; STEM DESIGN: NON RISING; STYLE: 1 WAY; TEMPERATURE RATING: 20 K; PORT TYPE: STANDARD; APPLICATION: TURBINE; SPECIFICATION: ISO 9001; SPECIAL FEATURES: NONE; GRADE: 304; DESIGN RATING: JIS 20K","KITZ Corporation , Shoritsu (Japan) , Bestway Valve (China) , J-Valves Fluid Equipment (China)","GATE; ISOLATING; STANDARD","250 MM","STAINLESS STEEL","JIS 20K; 2-2.8 MPA","HF; NON RISING","FLANGE","455 MM","N/A","ACTUATOR","TURBINE","20 K; 220-350 DEG C"]
["0620405","VALVE, BALL: VALVE SIZE: 200 MM; DESIGN RATING: JIS 10 K; TEMPERATURE RATING: 10 K; CONNECTION: FLANGE; BODY MATERIAL: SS GR 304; FACE TO FACE LENGTH: 455 MM; OPERATED: ACTUATOR, HANDWHEEL; STYLE: 1 WAY; SOFTGOODS: PTFE; APPLICATION: GENERATOR; TYPE: ISOLATING; .","PISTER,SAMSUNG","BALL; ISOLATING","200 MM","SS GR 304","JIS 10 K","STAINLESS STEEL BALL","FLANGE","455 MM","N/A","ACTUATOR, HANDWHEEL","GENERATOR","10 K"]
["0620407","VALVE, GLOBE: VALVE SIZE: 50 MM; FACE TO FACE LENGTH: 200 MM; OPERATED: HANDWHEEL; CONNECTION: FLANGE; BODY MATERIAL: SCS13; TRIM: SS GR 304; STEM DESIGN: RISING; STYLE: 1 WAY; APPLICATION: DRAIN; TYPE: ISOLATING; DESIGN RATING: JIS 20K; TEMPERATURE RATING: 20K","KITZ Corporation , Shoritsu (Japan) , Bestway Valve (China) , J-Valves Fluid Equipment (China)","GLOBE; ISOLATING","50 MM","SCS13","JIS 20K","SS GR 304; RISING","FLANGE","200 MM","N/A","HANDWHEEL","DRAIN","20K"]
["0620408","VALVE, GLOBE: VALVE SIZE: 2 IN; FACE TO FACE LENGTH: 200 MM; OPERATED: HANDWHEEL; CONNECTION: FLANGE; BODY MATERIAL: A105; TRIM: 13CR; STEM DESIGN: RISING; STYLE: 1 WAY; APPLICATION: DRAIN; TYPE: ISOLATING; DESIGN RATING: JIS 10K; TEMPERATURE RATING: 840 DEG F","KITZ Corporation , Shoritsu (Japan) , Bestway Valve (China) , J-Valves Fluid Equipment (China)","GLOBE; ISOLATING","2 IN","A105","JIS 10K","13CR; RISING","FLANGE","200 MM","N/A","HANDWHEEL","DRAIN","840 DEG F"]
["0628662","VALVE: TYPE: SAFETY; VALVE SIZE: 4 IN; DESIGN RATING: 53 BAR; TEMPERATURE RATING: 538 DEG C; CONNECTION: FLANGE; OPERATED: PRESSURE, SPRING, 0-35 LB; BODY MATERIAL: BS 1504-240; STYLE: ANGLE PATTERN; TRIM: PT; OEM P/N: 4\"707 SD; DRAWING NO: F5217/5 REV 0; .","LESER","SAFETY","4 IN","BS 1504-240","53 BAR","PT","FLANGE","150 MM- 240 MM","N/A","PRESSURE, SPRING, 0-35 LB","VARIOUS","538 DEG C"]
["0628694","VALVE, BALL: VALVE SIZE: 50 MM; DESIGN RATING: 63 BAR; TEMPERATURE RATING: 200 DEG C; CONNECTION: FEMALE THD; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 140 MM; OPERATED: HAND; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: PTFE; SPECIFICATION: JT97AN; PORT TYPE: BALL; APPLICATION: VARIOUS; GRADE: 1.4408; TYPE: ISOLATING","PISTER,PARKER,HYDEC","BALL; ISOLATING","50 MM","STAINLESS STEEL","63 BAR","STAINLESS STEEL","FEMALE THD","140 MM","N/A","HAND","VARIOUS","200 DEG C"]
["0628697","VALVE, RELIEF: VALVE SIZE: 3/4 IN; SET PRESSURE: 47.2 BAR; TEMPERATURE RATING: -10 TO 100 DEG C; CONNECTION: THREADED FEMALE; BODY MATERIAL: BRASS; TRIM: BRASS; FACE TO FACE LENGTH: 118 MM; OPERATED: PRESSURE; ORIFICE SIZE: 10 MM; SPECIFICATION: ISO 4126-1; APPLICATION: VARIOUS; STYLE: 1 WAY; SOFTGOODS: BRASS; DESIGN RATING: 150 BAR; PRESSURE RANGE: 42-25 BAR; MANUF P/N: H10N11787","LESER, REXROTH","RELIEF","3/4 IN; 10 MM","BRASS","150 BAR; 42-25 BAR; 47.2 BAR","BRASS","THREADED FEMALE","118 MM","N/A","PRESSURE","VARIOUS","-10 TO 100 DEG C"]
["0637382","VALVE: TYPE: CONCENTRIC; VALVE SIZE: OD 225 X THK 30 MM; DESIGN RATING: 380 BAR; TEMPERATURE RATING: -28 TO 425 DEG C; CONNECTION: SEAT; OPERATED: MECHANICAL; BODY MATERIAL: STAINLESS STEEL; STYLE: LEAF; MANUF P/N: 37134; MODEL NO: WP6310; FOR USE ON JP SAUER AND SOHN COMPRESSOR","SAUER COMPRESSOR","CONCENTRIC","OD 225 X THK 30 MM","STAINLESS STEEL","380 BAR","STAINLESS STEEL","SEAT","N/A","N/A","MECHANICAL","JP SAUER AND SOHN COMPRESSOR","-28 TO 425 DEG C"]
["0637420","VALVE, BALL: VALVE SIZE: DN 50; DESIGN RATING: PN100; TEMPERATURE RATING: 0-30 DEG C; CONNECTION: FLANGE; BODY MATERIAL: 1.4571; OPERATED: LEVER; SPECIFICATION: SAE; DIN; ANSI; ISO; TYPE: HYDRAULIC; REFERENCE NO: 190-050-138","PISTER, PARKER,HYDEC","BALL; HYDRAULIC","DN 50","1.4571","PN100","STAINLESS STEEL","FLANGE","N/A","N/A","LEVER","HYDRAULIC OIL SERVICE","0-30 DEG C"]
["0637421","VALVE, BALL: VALVE SIZE: DN 100; DESIGN RATING: PN100; TEMPERATURE RATING: -10 TO 50 DEG C; CONNECTION: FLANGE; BODY MATERIAL: 1.4571; OPERATED: LEVER; SPECIFICATION: SAE; DIN; ANSI; ISO; TYPE: PNEUMATIC; REFERENCE NO: 190-100-202; .","PARKER, HYDEC, VALVES FOR AFRICA","BALL; PNEUMATIC","DN 100","1.4571","PN100","STAINLESS","FLANGE","230 MM","235 MM","LEVER","COMPRESSED AIR, PNEUMATIC GAS SERVICE (CLEAN, DRY, HIGH-PRESSURE GAS SYSTEM","-10 TO 50 DEG C"]
["0637560","VALVE, RELIEF: VALVE SIZE: 1 IN; SET PRESSURE: 88 BAR; TEMPERATURE RATING: 0-50 DEG C; CONNECTION: G1 IN-BSPP; BODY MATERIAL: STAINLESS STEEL; TRIM: STAINLESS STEEL; FACE TO FACE LENGTH: L SHAPE; OPERATED: AIR; ORIFICE SIZE: 1 IN; SPECIFICATION: GL1238640; APPLICATION: COMPRESSOR; GRADE: 316; STYLE: 1 WAY; SOFTGOODS: STAINLESS STEEL; DESIGN RATING: 88 BAR G; PRESSURE RANGE: IN PN 250; OUT PN 40; MANUF P/N: M33H03X00V56V66J23H01","LESER,REXROTH,ENERGY VALVES,VOITH","RELIEF","1 IN","STAINLESS STEEL","88 BAR G; IN PN 250; 88 BAR","STAINLESS STEEL","G1 IN-BSPP","L SHAPE","N/A","AIR","COMPRESSOR","0-50 DEG C"]
["0637562","VALVE, RELIEF: VALVE SIZE: 1/2 IN; SET PRESSURE: 3 BAR; TEMPERATURE RATING: 0-20 DEG C; CONNECTION: THD 1/2 IN; BODY MATERIAL: STAINLESS STEEL; TRIM: STAINLESS STEEL; FACE TO FACE LENGTH: L SHAPE; OPERATED: AIR; ORIFICE SIZE: 1 IN; SPECIFICATION: 14/980; APPLICATION: COMPRESSOR; GRADE: 316; STYLE: 1 WAY; SOFTGOODS: STAINLESS STEEL; DESIGN RATING: 3 BAR; PRESSURE RANGE: IN PN 250; OUT PN 160; MANUF P/N: M33H03X00V54V65; .","LESER,REXROTH,ENERGY VALVES,VOITH","RELIEF","1/2 IN; 1 IN","STAINLESS STEEL","3 BAR; IN PN 250","STAINLESS STEEL","THD 1/2 IN","L SHAPE","N/A","AIR","COMPRESSOR","0-20 DEG C"]
["0638401","VALVE, BALL: VALVE SIZE: 1/2 IN; DESIGN RATING: PN30; TEMPERATURE RATING: 0-200 DEG C; CONNECTION: FEMALE THD; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 59 MM; OPERATED: LEVER; STYLE: 1 WAY; TRIM: BRASS; SOFTGOODS: NYLON; APPLICATION: FIRE SYSTEM; GRADE: 316; TYPE: LOCKABLE; MANUF P/N: 1610LD210","PISTER, PARKER,HYDEC","BALL; LOCKABLE","1/2 IN","STAINLESS STEEL","PN30","BRASS","FEMALE THD","59 MM","N/A","LEVER","FIRE SYSTEM","0-200 DEG C"]
["0638405","VALVE, ANGLE: TYPE: SUPPLY; VALVE SIZE: 80 MM; DESIGN RATING: 50 BAR; TEMPERATURE RATING: 300 DEG C; CONNECTION: THD FEMALE; BODY MATERIAL: BRASS; FACE TO FACE LENGTH: RIGHT ANGLE; OPERATED: HANDWHEEL; STYLE: 1 WAY; TRIM: RUBBER/SS; SOFTGOODS: BRASS; APPLICATION: FIRE HYDRANT; REFERENCE NO: VA001; KRS FIRE.","Krs Fire","ANGLE; SUPPLY","80 MM","BRASS","50 BAR","RUBBER/SS","THD FEMALE","RIGHT ANGLE","N/A","HANDWHEEL","FIRE HYDRANT","300 DEG C"]
["0642473","VALVE: TYPE: DIRECTIONAL; VALVE SIZE: 8/4 MM; DESIGN RATING: 350 BAR; TEMPERATURE RATING: 52 DEG C; FACE TO FACE LENGTH: 49 MM; CONNECTION: BOLT BLOCK; OPERATED: PRESSURE; BODY MATERIAL: STEEL; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SPECIFICATION: ISO 4401-03; SOFTGOODS: NBR; SPECIAL FEATURES: NIL; MANUF P/N: WDMFA06-AB3-G220/MD-HF1-P1AB",null,"DIRECTIONAL","8/4 MM","STEEL","350 BAR","STAINLESS STEEL","BOLT BLOCK","49 MM",null,"PRESSURE",null,"52 DEG C"]
["0643976","VALVE, BALL: VALVE SIZE: DN 50; DESIGN RATING: PN200; TEMPERATURE RATING: 180 DEG C; CONNECTION: THD; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 140 MM; OPERATED: LEVER; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: PTFE; SPECIFICATION: ISO 9001; PORT TYPE: FULL BORE; APPLICATION: VARIOUS; GRADE: 1.4408; TYPE: LOCKABLE; BODY SHAPE: SQUARE","PISTER,PARKER,HYDEC, VALVE  FOR AFRICA","BALL; FULL BORE; LOCKABLE","DN 50","STAINLESS STEEL","PN200","STAINLESS STEEL","THD","140 MM","N/A","LEVER","VARIOUS","180 DEG C"]
["0643977","VALVE, BALL: VALVE SIZE: 12 MM; DESIGN RATING: PN500; TEMPERATURE RATING: 180 DEG C; CONNECTION: 18L; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 115 MM; OPERATED: LEVER; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: NBR; SPECIFICATION: ISO 9001; PORT TYPE: FULL BORE; APPLICATION: VARIOUS; GRADE: 1.4571; TYPE: NON LOCKABLE; MANUF P/N: KH 18L-71X; BODY SHAPE: SQUARE","PISTER, PAKER, KLINGER MZANSI","BALL; FULL BORE; NON LOCKABLE","12 MM","STAINLESS STEEL","PN500","STAINLESS STEEL","18L","115 MM","N/A","LEVER","VARIOUS","180 DEG C"]
["0643978","VALVE, BALL: VALVE SIZE: 1/2 IN; DESIGN RATING: PN500; TEMPERATURE RATING: 180 DEG C; CONNECTION: THD; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 90 MM; OPERATED: LEVER; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: PTFE; SPECIFICATION: ISO 9001; PORT TYPE: FULL BORE; APPLICATION: VARIOUS; GRADE: 1.4423; TYPE: NON LOCKABLE; MANUF P/N: KH 1/2IN 71X; BODY SHAPE: SQUARE","KLINGER MZANSI, MAJOR VALVES, VALVES FOR AFRICA, PISTER, PAKER","BALL; FULL BORE; NON LOCKABLE","1/2 IN","STAINLESS STEEL","PN500","STAINLESS STEEL","THD","90 MM","N/A","LEVER","VARIOUS","180 DEG C"]
["0643979","VALVE: TYPE: SHUT OFF; VALVE SIZE: DN 4; DESIGN RATING: PN250; TEMPERATURE RATING: 250 DEG C; FACE TO FACE LENGTH: 105 MM; CONNECTION: THD G1/2 IN; OPERATED: HANDWHEEL; BODY MATERIAL: BRASS; STYLE: 1 WAY; TRIM: BRASS; GRADE: C360; SPECIFICATION: ISO 9001; SOFTGOODS: BRASS; SPECIAL FEATURES: GAUGE/TRANSMITTER FITTING","BMG (BEARING MAN GROUP), AXIOM HYDRAULICS, HYTEC GROUP, VALUE AND AUTOMATION (PTY) LTD, SWAGELOK SOUTH AFRICA","SHUT OFF","DN 4","BRASS","PN250","BRASS","THD G1/2 IN","105 MM","N/A","HANDWHEEL","INSTRUMENTATION SERVICE-PRIMARILY COMPRESSED AIR OR NON- CORROSIVE FLUIDS USED FOR PRESSURE GAUGE AND TRANSMITTER ISOLATION","250 DEG C"]
["0644949","VALVE, RELIEF: VALVE SIZE: 10 MM; SET PRESSURE: 65 BAR; TEMPERATURE RATING: -30 TO 80 DEG C; CONNECTION: THREADED; BODY MATERIAL: STEEL; TRIM: METAL; FACE TO FACE LENGTH: 80 MM; OPERATED: PRESSURE; ORIFICE SIZE: 5 MM; SPECIFICATION: ISO 9001; APPLICATION: VARIOUS; GRADE: 913000149; STYLE: 1 WAY; SOFTGOODS: NBR; DESIGN RATING: 25-400 BAR; PRESSURE RANGE: 0-630 BAR; MANUF P/N: R901260712; MODEL NO: DBDS 10 G19/65E","REXROTH","RELIEF","10 MM; 5 MM","STEEL","25-400 BAR; 0-630 BAR; 65 BAR","METAL","THREADED","80 MM","N/A","PRESSURE","VARIOUS","-30 TO 80 DEG C"]
["0644951","VALVE, RELIEF: VALVE SIZE: 30 MM; SET PRESSURE: 130 BAR; TEMPERATURE RATING: -30 TO 80 DEG C; CONNECTION: SUBPLATE; BODY MATERIAL: STEEL; TRIM: METAL; FACE TO FACE LENGTH: 80 MM; OPERATED: PRESSURE; ORIFICE SIZE: 15 MM; SPECIFICATION: ISO 9001; APPLICATION: VARIOUS; GRADE: 913000149; STYLE: 1 WAY; SOFTGOODS: NBR; DESIGN RATING: 25-400 BAR; PRESSURE RANGE: 0-350 BAR; MANUF P/N: R901341824; MODEL NO: DBDS 30 G1A/130E","REXROTH","RELIEF","30 MM; 15 MM","STEEL","25-400 BAR; 0-350 BAR; 130 BAR","METAL","SUBPLATE","80 MM","N/A","PRESSURE","VARIOUS","-30 TO 80 DEG C"]
["0644953","VALVE, RELIEF: VALVE SIZE: 20 MM; SET PRESSURE: 100 BAR; TEMPERATURE RATING: -30 TO 80 DEG C; CONNECTION: SUBPLATE; BODY MATERIAL: STEEL; TRIM: METAL; FACE TO FACE LENGTH: NIL; OPERATED: PRESSURE; ORIFICE SIZE: 10 MM; SPECIFICATION: ISO 9001; APPLICATION: VARIOUS; GRADE: 913000149; STYLE: 1 WAY; SOFTGOODS: NBR; DESIGN RATING: 25-400 BAR; PRESSURE RANGE: 10-350 BAR; MANUF P/N: R900597283; MODEL NO: DR 20-5-52/100YM","REXROTH","RELIEF","20 MM; 10 MM","STEEL","25-400 BAR; 10-350 BAR; 100 BAR","METAL","SUBPLATE","NIL","N/A","PRESSURE","VARIOUS","-30 TO 80 DEG C"]
["0647409","VALVE, SOLENOID: PIPE SIZE: 6 X 4 MM; STYLE: 3/2 WAY; POTENTIAL: 230 VAC; DESIGN RATING: 0-10 BAR; CONNECTION: G1/8 IN-BSPP; BODY MATERIAL: BRASS; OPERATED: AIR; ENCLOSURE RATING: IP65; MEDIUM: NATURAL GASES; FLUIDS; POWER: 8 W; ORIFICE SIZE: 2 MM; COIL: POLYAMIDE; SOFTGOODS: FKM; APPLICATION: FIRE DAMPER",null,"SOLENOID","6 X 4 MM; 2 MM","BRASS","0-10 BAR",null,"G1/8 IN-BSPP",null,null,"AIR","NATURAL GASES; FIRE DAMPER"]
["0648284","VALVE: TYPE: EMERGENCY CLOSING; VALVE SIZE: 13 MM; DESIGN RATING: 350 BAR; TEMPERATURE RATING: 200 DEG C; FACE TO FACE LENGTH: FLAT; CONNECTION: THREADED; OPERATED: PRESSURE; BODY MATERIAL: STEEL; STYLE: 2 WAY; SPECIFICATION: ISO 9001; TURBINE GOVERNOR PUMP CONTROL; KKS: MFX20AA201/219","VOITH","EMERGENCY CLOSING","13 MM","STEEL","350 BAR","POPPET (CLOSURE ELEMENT), VALVE SEAT, PRESSURE-ACTUATED PISTON/DIAPHRAM, RETURN SPRING (FAIL-SAFE), GUIDE BUSHINGS, INTERNAL SEALS AND FLOW PASSAGES.","THREADED","FLAT","N/A","PRESSURE","HIGH-PRESSURE HYDRAULIC/CONTROL OIL SERVICE USED IN TURBINE GOVERNOR AND PUMP CONTROL SYSTEMS FOR EMERGENCY SHUTOFF APPLICATIONS","200 DEG C"]
["0655228","VALVE, RELIEF: VALVE SIZE: G1/2 IN; SET PRESSURE: 365 KPA; TEMPERATURE RATING: -10 TO 220 DEG C; CONNECTION: G1/2 IN; BODY MATERIAL: 1.4104 (430); TRIM: METAL; FACE TO FACE LENGTH: 46 MM; OPERATED: PRESSURE; ORIFICE SIZE: 10 MM; SPECIFICATION: DIN ISO 228-1; APPLICATION: VARIOUS; GRADE: 1.4104; STYLE: 1 WAY; SOFTGOODS: 1.4404; DESIGN RATING: PN160-400; PRESSURE RANGE: 180-365 BAR; MANUF P/N: 4373.2602; REFERENCE NO: D0 10-D/G 0.5 F 0.35; .","REXROTH","RELIEF","G1/2 IN; 10 MM","1.4104 (430)","PN160-400; 180-365 BAR; 365 KPA","METAL","G1/2 IN","46 MM","N/A","PRESSURE","VARIOUS","-10 TO 220 DEG C"]
["0692543","VALVE: TYPE: NON RETURN; VALVE SIZE: 20 MM; TEMPERATURE RATING: -10 TO 100 DEG C; CONNECTION: 1/2 IN-BSP; OPERATED: AIR; BODY MATERIAL: STAINLESS STEEL; OEM P/N: 033930","SAUER,BOGE","NON RETURN","20 MM","STAINLESS STEEL","90BAR","S/S","1/2 IN-BSP","N/A","N/A","AIR","COMPRESSED AIR","-10 TO 100 DEG C"]
["0692898","VALVE, SOLENOID: PIPE SIZE: 1/2 IN; STYLE: 1/1; POTENTIAL: 220 VDC; DESIGN RATING: 0-1.5 MPA; CONNECTION: BSPF; BODY MATERIAL: BRASS; OPERATED: SOLENOID; ENCLOSURE RATING: IP65; MEDIUM: AIR; ORIFICE SIZE: 3 MM; COIL: SINGLE; APPLICATION: MECHANICAL AIR BRAKE SYSTEM; OEM P/N: VS3P-4030-10G HMJ-X",null,"SOLENOID","1/2 IN; 3 MM","BRASS","0-1.5 MPA",null,"BSPF",null,null,"SOLENOID","AIR; MECHANICAL AIR BRAKE SYSTEM"]
["0694573","VALVE, SOLENOID: PIPE SIZE: 1 IN; STYLE: 1/1; POTENTIAL: 24 VDC; DESIGN RATING: 10 BAR; CONNECTION: FNPT; BODY MATERIAL: STAINLESS STEEL; OPERATED: COIL SOLENOID VALVE; ENCLOSURE RATING: IP65; MEDIUM: DIESEL; ORIFICE SIZE: 15-25 MM; COIL: SINGLE; SOFTGOODS: O RING; APPLICATION: DIESEL; MODEL NO 2W-160-15, BOTH VALVE PORT; SIZE 1 IN",null,"SOLENOID","1 IN; 15-25 MM","STAINLESS STEEL","10 BAR",null,"FNPT",null,null,"COIL SOLENOID VALVE","DIESEL"]
[715945,"VALVE, CHECK: TYPE: NON-RETURN; VALVE SIZE: 650 MM; DESIGN RATING: Y 0.35 AND VACUUM MPA; TEMPERATURE RATING: 200 DEG C; CONNECTION: BUTT-WELDED; BODY MATERIAL: STEEL ASTM A216-WCB; FACE TO FACE LENGTH: 1448 MM; OPERATED: AUTO; TRIM: STEEL; APPLICATION: CHECK VALVE LBS30AA501; SPECIFICATION: ANSI B16 34 CLASS 150; DRAWING NO: FB21EV650NFDA ITEM DEWRANCE; BLED STEAM CHECK VALVE, BODY: WBC, SEAT: CR13, DISK: CR18","Dewrance","CHECK; BODY; NON-RETURN","650 MM","STEEL ASTM A216-WCB","Y 0.35 AND VACUUM MPA","STEEL","BUTT-WELDED","1448 MM","914 MM, 20 HOLES","AUTO","CHECK VALVE LBS30AA501","200 DEG C"]
["0726792","VALVE, SOLENOID: PIPE SIZE: 28 MM; STYLE: COAXIAL 3/2 WAY DIRECT ACTING; POTENTIAL: 230 VAC; DESIGN RATING: 100 BAR; CONNECTION: G3/4 IN FEMALE; BODY MATERIAL: BRASS; OPERATED: SOLENOID; ENCLOSURE RATING: IP65; MEDIUM: AIR; POWER: 0.4 W; CURRENT: 0.15 A; ORIFICE SIZE: 15 MM; SOFTGOODS: NBR ORING; APPLICATION: DRAIN VALVE; MANUF P/N: 039599; STAGE 3 DRAIN VALVE","Coax","SOLENOID","28 MM; 15 MM","BRASS","100 BAR","BRASS AND STAINLESS STEEL INTERNAL COMPONENTS WITH NBR SEALING ELEMENTS","G3/4 IN FEMALE","140 MM - 160 MM","N/A","SOLENOID","AIR; DRAIN VALVE","120°C - 400°C"]
["0628695","VALVE, BALL: VALVE SIZE: 20 MM; DESIGN RATING: 40 BAR; TEMPERATURE RATING: 200 DEG C; CONNECTION: FLANGED; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 44 MM; OPERATED: HAND; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: PTFE; SPECIFICATION: K6HT; PORT TYPE: BALL; APPLICATION: VARIOUS; GRADE: 1.4408; TYPE: ISOLATING","KLINGER MZANSI, RHYNO VALVES,PARKER","BALL; ISOLATING","20 MM","STAINLESS STEEL","40 BAR","STAINLESS STEEL","FLANGED","44 MM",null,"HAND","VARIOUS","200 DEG C"]
["0620405","VALVE, BALL: VALVE SIZE: 200 MM; DESIGN RATING: JIS 10 K; TEMPERATURE RATING: 10 K; CONNECTION: FLANGE; BODY MATERIAL: SS GR 304; FACE TO FACE LENGTH: 455 MM; OPERATED: ACTUATOR, HANDWHEEL; STYLE: 1 WAY; SOFTGOODS: PTFE; APPLICATION: GENERATOR; TYPE: ISOLATING; .","PARKER, HYDEC, VALVES FOR AFRICA","BALL; ISOLATING","200 MM","SS GR 304","JIS 10 K","BALL, STEM, GLAND PACKING FOLLOWER (STAINLESS STEEL), SEALS, PACKING (PTFE)","FLANGE","455 MM","75 MM","ACTUATOR, HANDWHEEL","GENERATOR","10 K"]
["0620406","VALVE, BALL: VALVE SIZE: 200 MM; DESIGN RATING: JIS 10 K; TEMPERATURE RATING: 10 K; CONNECTION: FLANGE; BODY MATERIAL: SS GR 304; FACE TO FACE LENGTH: 455 MM; OPERATED: ACTUATOR, CHAIN; STYLE: 1 WAY; SOFTGOODS: PTFE; APPLICATION: GENERATOR; TYPE: ISOLATING","PARKER, PISTER, KLINGER MZANSI","BALL; ISOLATING","200 MM","SS GR 304","JIS 10 K","STAINLESS STEEL","FLANGE","455 MM","340 MM","ACTUATOR, CHAIN","GENERATOR","10 K"]
["0692543","VALVE: TYPE: NON RETURN; VALVE SIZE: 20 MM; TEMPERATURE RATING: -10 TO 100 DEG C; CONNECTION: 1/2 IN-BSP; OPERATED: AIR; BODY MATERIAL: STAINLESS STEEL; OEM P/N: 033930","SAUER COMPRESSOR, BOGE","NON RETURN","20 MM","STAINLESS STEEL","90bar","s/s","1/2 IN-BSP","60 MM","N/A","AIR","AIR, WATER, GENERAL INDISTRIAL FLUIDS","-10 TO 100 DEG C"]
["0628696","VALVE, BALL: VALVE SIZE: 1/2 IN; DESIGN RATING: 2000 KPA; TEMPERATURE RATING: 200 DEG C; CONNECTION: FEMALE THD; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 75 MM; OPERATED: HAND; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: PTFE; SPECIFICATION: 5BDB 5BEE; PORT TYPE: BALL; APPLICATION: VARIOUS; GRADE: 1.4408; TYPE: ISOLATING; MANUF P/N: CF8M","PARKER, PISTER, KLINGER MZANSI","BALL; ISOLATING","1/2 IN","STAINLESS STEEL","2000 KPA","STAINLESS STEEL","FEMALE THD","75 MM","N/A","HAND","VARIOUS","200 DEG C"]
["0643978","VALVE, BALL: VALVE SIZE: 1/2 IN; DESIGN RATING: PN500; TEMPERATURE RATING: 180 DEG C; CONNECTION: THD; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 90 MM; OPERATED: LEVER; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: PTFE; SPECIFICATION: ISO 9001; PORT TYPE: FULL BORE; APPLICATION: VARIOUS; GRADE: 1.4423; TYPE: NON LOCKABLE; MANUF P/N: KH 1/2IN 71X; BODY SHAPE: SQUARE","PARKER, PISTER, KLINGER MZANSI","BALL; FULL BORE; NON LOCKABLE","1/2 IN","STAINLESS STEEL","PN500","STAINLESS STEEL","THD","90 MM","N/A","LEVER","VARIOUS","180 DEG C"]
["0637420","VALVE, BALL: VALVE SIZE: DN 50; DESIGN RATING: PN100; TEMPERATURE RATING: 0-30 DEG C; CONNECTION: FLANGE; BODY MATERIAL: 1.4571; OPERATED: LEVER; SPECIFICATION: SAE; DIN; ANSI; ISO; TYPE: HYDRAULIC; REFERENCE NO: 190-050-138","PARKER, PISTER, KLINGER MZANSI","BALL; HYDRAULIC","DN 50","1.4571","PN100","STAINLESS STEEL BALL AND BALL WITH PTFE SEATS AND PACKING, REINFORCED SEALING ELEMENTS SUITABLE FOR HIGH- PRESSURE HYDRAULIC SERVICE","FLANGE","150 MM","125 MM","LEVER","HYDRAULIC FLUID, WATER BASED FLUID, LIGHT GASE AND CHEMICALS","0-30 DEG C"]
["0643976","VALVE, BALL: VALVE SIZE: DN 50; DESIGN RATING: PN200; TEMPERATURE RATING: 180 DEG C; CONNECTION: THD; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 140 MM; OPERATED: LEVER; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: PTFE; SPECIFICATION: ISO 9001; PORT TYPE: FULL BORE; APPLICATION: VARIOUS; GRADE: 1.4408; TYPE: LOCKABLE; BODY SHAPE: SQUARE","PARKER, PISTER, KLINGER MZANSI","BALL; FULL BORE; LOCKABLE","DN 50","STAINLESS STEEL","PN200","STAINLESS STEEL","THD","140 MM","N/A","LEVER","VARIOUS","180 DEG C"]
["0657951","VALVE, BALL: VALVE SIZE: DN 80; DESIGN RATING: PN100; TEMPERATURE RATING: 0-30 DEG C; CONNECTION: FLANGE; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 160 MM; OPERATED: ACTUATOR; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: PTFE; SPECIFICATION: ISO 9001; PORT TYPE: SCREW; APPLICATION: TURBINE; GRADE: 1.4301; TYPE: SHUT OFF; MODEL NO: FCKH; REFERENCE NO: 9423 107/15; PISTER","PARKER, PISTER, KLINGER MZANSI","BALL; SCREW; SHUT OFF","DN 80","STAINLESS STEEL","PN100","STAINLESS STEEL","FLANGE","160 MM","160 MM","ACTUATOR","TURBINE","0-30 DEG C"]
["0657952","VALVE, BALL: VALVE SIZE: DN 80; DESIGN RATING: PN100; TEMPERATURE RATING: 0-40 DEG C; CONNECTION: FLANGE; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 160 MM; OPERATED: ACTUATOR/LEVER; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: PTFE; SPECIFICATION: ISO 9001; PORT TYPE: SCREW; APPLICATION: TURBINE; GRADE: 1.4301; TYPE: SHUT OFF; MODEL NO: FCKH; REFERENCE NO: 9423 279/13; COMPLETE WITH EXTENSION; PISTER","PARKER, PISTER, VOITH","BALL; SCREW; SHUT OFF","DN 80","STAINLESS STEEL","PN100","STAINLESS STEEL","FLANGE","160 MM","160 MM","ACTUATOR/LEVER","TURBINE","0-40 DEG C"]
["0657953","VALVE, BALL: VALVE SIZE: DN 80; DESIGN RATING: PN100; TEMPERATURE RATING: 0-40 DEG C; CONNECTION: FLANGE; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 160 MM; OPERATED: ACTUATOR/LEVER; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: PTFE; SPECIFICATION: ISO 9001; PORT TYPE: SCREW; APPLICATION: TURBINE; GRADE: 1.4301; TYPE: SHUT OFF; MODEL NO: FCKH; REFERENCE NO: 9423 452/13; PISTER","PARKER, PISTER, VOITH","BALL; SCREW; SHUT OFF","DN 80","STAINLESS STEEL","PN100","STAINLESS STEEL","FLANGE","160 MM","160 MM","ACTUATOR/LEVER","TURBINE","0-40 DEG C"]
["0628693","VALVE, BALL: VALVE SIZE: 25 MM; DESIGN RATING: 63; TEMPERATURE RATING: 200 DEG C; CONNECTION: FEMALE THD; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 90 MM; OPERATED: HAND; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: PTFE; SPECIFICATION: JT97AN; PORT TYPE: BALL; APPLICATION: VARIOUS; GRADE: 1.4408; TYPE: ISOLATING","PARKER, PISTER, KLINGER MZANSI","BALL; ISOLATING","25 MM","STAINLESS STEEL","63","STAINLESS STEEL","FEMALE THD","90 MM","N/A","HAND","VARIOUS","200 DEG C"]
["0619983","VALVE, BALL: VALVE SIZE: 50 MM; DESIGN RATING: 10 KPA; TEMPERATURE RATING: JIS10K; CONNECTION: FLANGED; BODY MATERIAL: SCPH2/304; FACE TO FACE LENGTH: 175 MM; OPERATED: LEVER; STYLE: DIRECTIONAL; TRIM: STL; SOFTGOODS: PTFE; APPLICATION: UPPER OIL COOLER; TYPE: ISOLATING","PARKER, PISTER, KLINGER MZANSI","BALL; ISOLATING","50 MM","SCPH2/304","10 KPA","STL","FLANGED","175 MM","120 MM","LEVER","UPPER OIL COOLER","JIS10K"]
["0628694","VALVE, BALL: VALVE SIZE: 50 MM; DESIGN RATING: 63 BAR; TEMPERATURE RATING: 200 DEG C; CONNECTION: FEMALE THD; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 140 MM; OPERATED: HAND; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: PTFE; SPECIFICATION: JT97AN; PORT TYPE: BALL; APPLICATION: VARIOUS; GRADE: 1.4408; TYPE: ISOLATING","PARKER, PISTER, KLINGER MZANSI","BALL; ISOLATING","50 MM","STAINLESS STEEL","63 BAR","STAINLESS STEEL","FEMALE THD","140 MM","N/A","HAND","VARIOUS","200 DEG C"]
["0637421","VALVE, BALL: VALVE SIZE: DN 100; DESIGN RATING: PN100; TEMPERATURE RATING: -10 TO 50 DEG C; CONNECTION: FLANGE; BODY MATERIAL: 1.4571; OPERATED: LEVER; SPECIFICATION: SAE; DIN; ANSI; ISO; TYPE: PNEUMATIC; REFERENCE NO: 190-100-202; .","PARKER, PISTER, KLINGER MZANSI, VOITH","BALL; PNEUMATIC","DN 100","1.4571","PN100","STAINLESS STEEL","FLANGE","≈ 230 mm","190 MM","LEVER","HYDRAULIC AND PNEUMATIC SYSTEMS, WATER SERVICES, GASES, LIGHT CHEMICAL FLUIDS","-10 TO 50 DEG C"]
["0648284","VALVE: TYPE: EMERGENCY CLOSING; VALVE SIZE: 13 MM; DESIGN RATING: 350 BAR; TEMPERATURE RATING: 200 DEG C; FACE TO FACE LENGTH: FLAT; CONNECTION: THREADED; OPERATED: PRESSURE; BODY MATERIAL: STEEL; STYLE: 2 WAY; SPECIFICATION: ISO 9001; TURBINE GOVERNOR PUMP CONTROL; KKS: MFX20AA201/219","VOITH","EMERGENCY CLOSING","13 MM","STEEL","350 BAR","STAINLESS STEEL","THREADED","FLAT","N/A","PRESSURE","HIGH PRESSURE HYDRAULIC OIL, TURBINE GOVERNOR OIL SYSTEM","200 DEG C"]
["0646934","VALVE: TYPE: DIRECTIONAL; VALVE SIZE: NG 6; DESIGN RATING: 350 BAR; TEMPERATURE RATING: -25 TO 70 DEG C; FACE TO FACE LENGTH: FLANGE; CONNECTION: SUBPLATE; OPERATED: HAND; BODY MATERIAL: CARBON STEEL; STYLE: 4/2 WAY; TRIM: STAINLESS STEEL; SPECIFICATION: ISO 4401-03; SOFTGOODS: NBR; MANUF P/N: AH4Z60A/R-Z80",null,"DIRECTIONAL","NG 6","CARBON STEEL","350 BAR","STAINLESS STEEL","SUBPLATE","FLANGE",null,"HAND",null,"-25 TO 70 DEG C"]
["0642473","VALVE: TYPE: DIRECTIONAL; VALVE SIZE: 8/4 MM; DESIGN RATING: 350 BAR; TEMPERATURE RATING: 52 DEG C; FACE TO FACE LENGTH: 49 MM; CONNECTION: BOLT BLOCK; OPERATED: PRESSURE; BODY MATERIAL: STEEL; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SPECIFICATION: ISO 4401-03; SOFTGOODS: NBR; SPECIAL FEATURES: NIL; MANUF P/N: WDMFA06-AB3-G220/MD-HF1-P1AB",null,"DIRECTIONAL","8/4 MM","STEEL","350 BAR","STAINLESS STEEL","BOLT BLOCK","49 MM",null,"PRESSURE",null,"52 DEG C"]
["0637416","VALVE: TYPE: SAFETY; VALVE SIZE: DN40; DESIGN RATING: 35 BAR; TEMPERATURE RATING: 20 DEG C; CONNECTION: FLANGE INLET P 40, OUTLET PN16; OPERATED: HAND LEVER; BODY MATERIAL: 1.4408; SPECIFICATION: 4414.4664; REFERENCE NO: 10944010; CENTER TO FACE: INLET 140 MM, OUTLET 115 MM","LESER,REXROTH,ENERGY VALVES,","SAFETY","DN40","1.4408","35 BAR","STAINLESS STEEL","FLANGE INLET P 40, OUTLET PN16","n/a","110 MM","HAND LEVER",null,"20 DEG C"]
["0630729","VALVE: TYPE: ISOLATING GAUGE; VALVE SIZE: DN 4; DESIGN RATING: PN400; TEMPERATURE RATING: -20 TO 200 DEG C; FACE TO FACE LENGTH: 140 MM; CONNECTION: THD MALE X FEMALE; OPERATED: HANDWHEEL; BODY MATERIAL: STAINLESS STEEL; STYLE: 2 WAY; GRADE: 1.4571; SPECIAL FEATURES: VENT SCREW","PAKER, SUPERPUMP , HYDRAULICS, PISTER","ISOLATING GAUGE","DN 4","STAINLESS STEEL","PN400","STAINLESS STEEL","THD MALE X FEMALE","140 MM","N/A","HANDWHEEL",null,"-20 TO 200 DEG C"]
["0630728","VALVE: TYPE: ISOLATING GAUGE; VALVE SIZE: DN 4; TEMPERATURE RATING: -20 TO 200 DEG C; FACE TO FACE LENGTH: 140 MM; CONNECTION: THD MALE X FEMALE; OPERATED: HANDWHEEL; BODY MATERIAL: STAINLESS STEEL; STYLE: 3 WAY; GRADE: 1.4571; SPECIAL FEATURES: VENT SCREW","PAKER, SUPERPUMP , HYDRAULICS, PISTER","ISOLATING GAUGE","DN 4","STAINLESS STEEL","PN400","STAINLESS STEEL","THD MALE X FEMALE","140 MM","N/A","HANDWHEEL","HYDRAULIC OIL","-20 TO 200 DEG C"]
["0072645","VALVE: TYPE: HYDRAULIC; VALVE SIZE: 3/4 IN","PISTER/UFIXED/HYDEC","HYDRAULIC","3/4 IN","STAINLESS STEEL","PN315","STAINLESS STEEL, ","THREADED","≈ 70 – 120 mm","N/A","MANUALLY","HYDRAULIC OIL","–20°C to +80°C"]
["0644906","VALVE, CHECK: TYPE: DUAL PURPOSE; VALVE SIZE: 1-1/2 IN; DESIGN RATING: 3000 PSI; TEMPERATURE RATING: -30 TO 80 DEG C; CONNECTION: INSERT; BODY MATERIAL: STEEL; FACE TO FACE LENGTH: 65 MM; OPERATED: PRESSURE; STYLE: 1 WAY; TRIM: BRASS; SOFTGOODS: NITRILE; APPLICATION: SAE FLANGE PORT; SPECIFICATION: ISO 9001; GRADE: HT; MANUF P/N: RVSAE3-112-5 13K","VALVES FOR AFRIKA,SUPERPUMP, KLINGER MZANSI","CHECK; DUAL PURPOSE","1-1/2 IN","STEEL","3000 PSI","BRASS","INSERT","65 MM","N/A","PRESSURE","SAE FLANGE PORT","-30 TO 80 DEG C"]
["0628680","VALVE, CHECK: TYPE: DISC; VALVE SIZE: DN 80; DESIGN RATING: PN40; TEMPERATURE RATING: -200 TO 550 DEG C; CONNECTION: FLANGE; BODY MATERIAL: CI 300; FACE TO FACE LENGTH: 50 MM; OPERATED: FLOW; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: STAINLESS STEEL; APPLICATION: VARIOUS; SPECIFICATION: (PED) 97/23/EC; GRADE: 1.4408; MANUF P/N: RK86A; WITH BODY CENTERING CAMS; FLOWSERVE","VALVES FOR AFRIKA,SUPERPUMP, KLINGER MZANSI","CHECK; DISC","DN 80","CI 300","PN40","STAINLESS STEEL","FLANGE","50 MM","160 mm","FLOW","VARIOUS","-200 TO 550 DEG C"]
["0644902","VALVE: TYPE: DIRECTIONAL PISTON; VALVE SIZE: NG10; DESIGN RATING: 315 BAR; TEMPERATURE RATING: -5 TO 50 DEG C; FACE TO FACE LENGTH: NIL; CONNECTION: MOUNTING PLATE; OPERATED: ELECTRIC; BODY MATERIAL: CAST IRON; STYLE: 4/2 WAY; TRIM: STAINLESS STEEL; GRADE: NIL; SPECIFICATION: ISO 9001; SOFTGOODS: NBR; SPECIAL FEATURES: NIL; MANUF P/N: WE02-10P100E220/CHN",null,"DIRECTIONAL PISTON","NG10","CAST IRON","315 BAR","STAINLESS STEEL","MOUNTING PLATE","NIL",null,"ELECTRIC",null,"-5 TO 50 DEG C"]
["0623858","VALVE, CHECK: TYPE: FLOW CONTROL; VALVE SIZE: NS16; DESIGN RATING: 1.5 BAR; TEMPERATURE RATING: -20 TO 80 DEG C; CONNECTION: FLANGE; BODY MATERIAL: CI; FACE TO FACE LENGTH: 70 MM; OPERATED: PILOT; STYLE: 2 WAY; APPLICATION: SURGE CHAMBER HOIST; SPECIFICATION: DIN 51524; OEM P/N: 2FRM16-32/160L, OEM: BOSCH REXROTH; LOCKABLE; FLOW RATE: 160 L/MIN.","Bosch; Rexroth","CHECK; FLOW CONTROL","NS16","CI","1.5 BAR","HARDENED STEEL","FLANGE","70 MM","N/A","PILOT","SURGE CHAMBER HOIST","-20 TO 80 DEG C"]
["0623859","VALVE, CHECK: TYPE: FLOW CONTROL; VALVE SIZE: NS10; DESIGN RATING: 1.5 BAR; TEMPERATURE RATING: -20 TO 80 DEG C; CONNECTION: FLANGE; BODY MATERIAL: CI; FACE TO FACE LENGTH: 55 MM; OPERATED: PILOT; STYLE: 2 WAY; APPLICATION: SURGE CHAMBER HOIST; SPECIFICATION: DIN 51524; OEM P/N: 2FRM10-31/50L, OEM: BOSCH REXROTH; LOCKABLE; FLOW RATE: 50 L/MIN.","Bosch; Rexroth","CHECK; FLOW CONTROL","NS10","CI","1.5 BAR","HARDENED STEEL","FLANGE","55 MM","N/A","PILOT","SURGE CHAMBER HOIST","-20 TO 80 DEG C"]
["0178003","VALVE, CHECK: VALVE SIZE: 100 MM; DESIGN RATING: 3-8 BAR; TEMPERATURE RATING: 50-100 DEG C; MANUF P/N: NINSSC 0100; .","SUPERPUMP, KLINGER MZANSI","CHECK","100 MM","CAST IRON AND DUCTILE","3-8 BAR","STAINLESS STEEL","FLANGE","≈ 350 MM","180 MM","VARIOUS","WATER, HOT WATER AND CLEAN INDUSTRIAL FLUIDS","50-100 DEG C"]
["0628204","VALVE, BUTTERFLY: TYPE: WAFER; VALVE SIZE: DN65; DESIGN RATING: 16 BAR; TEMPERATURE RATING: -40 TO 200 DEG C; CONNECTION: CENTER FLANGE; BODY MATERIAL: CI; FACE TO FACE LENGTH: 46 MM; OPERATED: LEVERLOCK; TRIM: STAINLESS STEEL; SOFTGOODS: NBR; APPLICATION: WATER; GRADE: 1.4409; SPECIFICATION: EN ISO 5211; STYLE: CENTERED DISC; SCHEDULE: EN 558 SERIES 20; SPECIAL FEATURES: NONE; MANUF P/N: Z011-A","SUPERPUMP, KLINGER MZANSI","BUTTERFLY; WAFER","DN65","CI","16 BAR","STAINLESS STEEL","CENTER FLANGE","46 MM","145 MM","LEVERLOCK","WATER","-40 TO 200 DEG C"]
["0643980","VALVE, BUTTERFLY: TYPE: WAFER; VALVE SIZE: DN40; DESIGN RATING: 16 BAR; TEMPERATURE RATING: 200 DEG C; CONNECTION: FLANGE; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 33 MM; OPERATED: LEVER; TRIM: STAINLESS STEEL; SOFTGOODS: EPDM; APPLICATION: BLOWDOWN; GRADE: 1.4408; SPECIFICATION: EN 1092-1; STYLE: 1 WAY; SPECIAL FEATURES: ADJUSTABLE POSITION; MANUF P/N: Z011-A; CF8M; EBRO","SUPERPUMP, KLINGER MZANSI","BUTTERFLY; WAFER","DN40","STAINLESS STEEL","16 BAR","STAINLESS STEEL","FLANGE","33 MM","110 MM","LEVER","BLOWDOWN","200 DEG C"]
["0623861","VALVE, CHECK: TYPE: FLOW CONTROL; VALVE SIZE: 1 IN; DESIGN RATING: 320 BAR; TEMPERATURE RATING: -20 TO 100 DEG C; CONNECTION: THD; BODY MATERIAL: STEEL; FACE TO FACE LENGTH: 117 MM; OPERATED: PRESSURE, 0 BAR; STYLE: 1 WAY; APPLICATION: SURGE CHAMBER HOIST; SPECIFICATION: EN 10083; OEM P/N: FT257/6 100 0 BAR; SPRING REMOVED","SUPERPUMP, KLINGER MZANSI","CHECK; FLOW CONTROL","1 IN","STEEL","320 BAR","STEEL AND HARDENED STEEL","THD","117 MM","N/A","PRESSURE, 0 BAR","SURGE CHAMBER HOIST","-20 TO 100 DEG C"]
["0692898","VALVE, SOLENOID: PIPE SIZE: 1/2 IN; STYLE: 1/1; POTENTIAL: 220 VDC; DESIGN RATING: 0-1.5 MPA; CONNECTION: BSPF; BODY MATERIAL: BRASS; OPERATED: SOLENOID; ENCLOSURE RATING: IP65; MEDIUM: AIR; ORIFICE SIZE: 3 MM; COIL: SINGLE; APPLICATION: MECHANICAL AIR BRAKE SYSTEM; OEM P/N: VS3P-4030-10G HMJ-X","VALVES FOR AFRIKA,SUPERPUMP, KLINGER MZANSI","SOLENOID","1/2 IN; 3 MM","BRASS","0-1.5 MPA","STAINLESS AND BRASS","BSPF","60 - 80 MM","PCD","SOLENOID","AIR; MECHANICAL AIR BRAKE SYSTEM","–10°C to +80°C"]
["0692543","VALVE: TYPE: NON RETURN; VALVE SIZE: 20 MM; TEMPERATURE RATING: -10 TO 100 DEG C; CONNECTION: 1/2 IN-BSP; OPERATED: AIR; BODY MATERIAL: STAINLESS STEEL; OEM P/N: 033930","SAUER COMPRESSOR","NON RETURN","20 MM","STAINLESS STEEL","PN16","STAINLESS STEEL ","1/2 IN-BSP","50 - 70 MM","N/A","AIR","COMPRESSED AIR","-10 TO 100 DEG C"]
["0628662","VALVE: TYPE: SAFETY; VALVE SIZE: 4 IN; DESIGN RATING: 53 BAR; TEMPERATURE RATING: 538 DEG C; CONNECTION: FLANGE; OPERATED: PRESSURE, SPRING, 0-35 LB; BODY MATERIAL: BS 1504-240; STYLE: ANGLE PATTERN; TRIM: PT; OEM P/N: 4\"707 SD; DRAWING NO: F5217/5 REV 0; .","LESER,REXROTH","SAFETY","4 IN","BS 1504-240","53 BAR","PT","FLANGE","320 - 400 MM","190 MM","PRESSURE, SPRING, 0-35 LB","STEAM","538 DEG C"]
["0619975","VALVE: TYPE: SHUT OFF; VALVE SIZE: 3/8 IN; DESIGN RATING: 200 BAR; TEMPERATURE RATING: -10 TO 120 DEG C; FACE TO FACE LENGTH: 55 MM; CONNECTION: BSP SCREW; OPERATED: HAND; BODY MATERIAL: BRASS; STYLE: 3 WAY; OEM P/N: CA200MP; TYPE ASK","ASK","SHUT OFF","3/8 IN","BRASS","200 BAR","STAINLESS STEEL","BSP SCREW","55 MM","N/A","HAND","HYDRAULIC OIL, COMPRESSED AIR","-10 TO 120 DEG C"]
["0041833","VALVE: TYPE: COMPRESSOR; VALVE SIZE: 175 MM; OPERATED: PRESSURE; BODY MATERIAL: STL; TRIM: DISC SS; 2ND STAGE CONCENTRIC","SAUER COMPRESSOR","COMPRESSOR","175 MM","STL","27BAR","DISC SS","N/A","N/A","N/A","PRESSURE","COMPRESSED AIR","50 DEG C"]
["0637382","VALVE: TYPE: CONCENTRIC; VALVE SIZE: OD 225 X THK 30 MM; DESIGN RATING: 380 BAR; TEMPERATURE RATING: -28 TO 425 DEG C; CONNECTION: SEAT; OPERATED: MECHANICAL; BODY MATERIAL: STAINLESS STEEL; STYLE: LEAF; MANUF P/N: 37134; MODEL NO: WP6310; FOR USE ON JP SAUER AND SOHN COMPRESSOR","SAUER COMPRESSOR","CONCENTRIC","OD 225 X THK 30 MM","STAINLESS STEEL","380 BAR","STAINLESS STEEL","SEAT","N/A","N/A","MECHANICAL","JP SAUER AND SOHN COMPRESSOR","-28 TO 425 DEG C"]
["0701459","VALVE: TYPE: CONTROL; VALVE SIZE: NG10; DESIGN RATING: 120 BAR; TEMPERATURE RATING: 20-60 DEG C; CONNECTION: FLANGE; OPERATED: CONTINUOUSLY; BODY MATERIAL: STEEL; STYLE: BLOCK CM2; PROFIBUS DP STANDARD I6C61158 R24KX2F3H592-BDK2D1 MODEL: D637-1033-0001",null,"CONTROL","NG10","STEEL","120 BAR",null,"FLANGE",null,null,"CONTINUOUSLY",null,"20-60 DEG C"]
["0644954","VALVE: TYPE: DIRECTIONAL CONTROL; VALVE SIZE: 6 MM; DESIGN RATING: 350 BAR; TEMPERATURE RATING: -30 TO 80 DEG C; FACE TO FACE LENGTH: NIL; CONNECTION: SUBPLATE; OPERATED: SOLENOID; BODY MATERIAL: STEEL; STYLE: 4/2 WAY; TRIM: METAL; SPECIFICATION: ISO 9001; SOFTGOODS: NBR; SPECIAL FEATURES: WITH RNEH5-162R11/22000E1 SUBPLATE; MANUF P/N: RPE3-06R11/22000E1",null,"DIRECTIONAL CONTROL","6 MM","STEEL","350 BAR","METAL","SUBPLATE","NIL",null,"SOLENOID",null,"-30 TO 80 DEG C"]
["0623860","VALVE, CHECK: TYPE: FLOW CONTROL; VALVE SIZE: 1-1/4 IN; DESIGN RATING: 320 BAR; TEMPERATURE RATING: -20 TO 100 DEG C; CONNECTION: THD; BODY MATERIAL: STEEL; FACE TO FACE LENGTH: 134.5 MM; OPERATED: PRESSURE, 1 BAR; STYLE: 1 WAY; APPLICATION: SURGE CHAMBER HOIST; SPECIFICATION: EN 10083; OEM P/N: FT257/6 114 1 BAR","SUPERSUMP, KLINGERMZANSI, VALVES FOR AFRICA","CHECK; FLOW CONTROL","1-1/4 IN","STEEL","320 BAR","HARDENED STEEL","THD","134.5 MM","N/A","PRESSURE, 1 BAR","SURGE CHAMBER HOIST","-20 TO 100 DEG C"]
["0731181","VALVE, CHECK: TYPE: E65; VALVE SIZE: DN25 MM; DESIGN RATING: PN40; TEMPERATURE RATING: -20to70 degree; CONNECTION: FLANGE; BODY MATERIAL: CAST IRON; FACE TO FACE LENGTH: 0.01 M; OPERATED: ELECTRICAL ACTUATOR","VALVES FOR AFRIKA,SUPERPUMP, KLINGER MZANSI","CHECK; E65","DN25 MM","CAST IRON","PN40","STAINLESS STEEL","FLANGE","0.01 M","85 MM","ELECTRICAL ACTUATOR","WATER","-20to70 degree"]
["0644907","VALVE, CHECK: TYPE: DUAL PURPOSE; VALVE SIZE: 2-1/2 IN; DESIGN RATING: 3000 PSI; TEMPERATURE RATING: -30 TO 80 DEG C; CONNECTION: INSERT; BODY MATERIAL: STEEL; FACE TO FACE LENGTH: 85 MM; OPERATED: PRESSURE; STYLE: 1 WAY; TRIM: BRASS; SOFTGOODS: NITRILE; APPLICATION: SAE FLANGE PORT; SPECIFICATION: ISO 9001; GRADE: HT; MANUF P/N: RVSAE3DS-212-4","PISTER, PAKER ,KLINGER MZANSI, SUPERPUMP","CHECK; DUAL PURPOSE","2-1/2 IN","STEEL","3000 PSI","BRASS","INSERT","85 MM","127 MM","PRESSURE","SAE FLANGE PORT","-30 TO 80 DEG C"]
["0655868","VALVE, BUTTERFLY: TYPE: WAFER; VALVE SIZE: 250 MM; DESIGN RATING: PN100; TEMPERATURE RATING: -20 TO 200 DEG F; CONNECTION: FLANGE; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 235 MM; OPERATED: HANDWHEEL/GEARBOX; TRIM: STAINLESS STEEL; SOFTGOODS: PTFE; APPLICATION: VARIOUS; GRADE: 1.4408; STYLE: 1 WAY; REFERENCE NO: 1-MF-A10-060 G00; COMPLETE WITH ROTORK GEARBOX AB880N; LEUSCH LTR43","PISTER, PAKER ,KLINGER MZANSI, SUPERPUMP, VALVES FOR AFRICA","BUTTERFLY; WAFER","250 MM","STAINLESS STEEL","PN100","STAINLESS STEEL","FLANGE","235 MM","405 MM","HANDWHEEL/GEARBOX","VARIOUS","-20 TO 200 DEG F"]
["0628207","VALVE, BUTTERFLY: TYPE: WAFER; VALVE SIZE: DN125; DESIGN RATING: 16 BAR; TEMPERATURE RATING: -40 TO 200 DEG C; CONNECTION: CENTER FLANGE; BODY MATERIAL: CI; FACE TO FACE LENGTH: 56 MM; OPERATED: LEVERLOCK; TRIM: STAINLESS STEEL; SOFTGOODS: NBR; APPLICATION: WATER; GRADE: 1.4409; SPECIFICATION: EN ISO 5211; STYLE: CENTERED DISC; SCHEDULE: EN 558 SERIES 20; SPECIAL FEATURES: NONE; MANUF P/N: Z011-A","PISTER, PAKER ,KLINGER MZANSI, SUPERPUMP,VALVES FOR AFRICA","BUTTERFLY; WAFER","DN125","CI","16 BAR","STAINLESS STEEL","CENTER FLANGE","56 MM","210 MM","LEVERLOCK","WATER","-40 TO 200 DEG C"]
["0628203","VALVE, BUTTERFLY: TYPE: WAFER; VALVE SIZE: DN 50; DESIGN RATING: 10 BAR; TEMPERATURE RATING: -40 TO 200 DEG C; CONNECTION: CENTER FLANGE; BODY MATERIAL: CI; FACE TO FACE LENGTH: 43 MM; OPERATED: LEVERLOCK; TRIM: STAINLESS STEEL; SOFTGOODS: NBR; APPLICATION: WATER; GRADE: 1.4409; SPECIFICATION: EN ISO 5211; STYLE: CENTERED DISC; SCHEDULE: EN 558 SERIES 20; SPECIAL FEATURES: NONE; MANUF P/N: Z011-A; .","PISTER, PAKER ,KLINGER MZANSI, SUPERPUMP,VALVES FOR AFTICA","BUTTERFLY; WAFER","DN 50","CI","10 BAR","STAINLESS STEEL","CENTER FLANGE","43 MM","125 MM","LEVERLOCK","WATER","-40 TO 200 DEG C"]
["0628205","VALVE, BUTTERFLY: TYPE: WAFER; VALVE SIZE: 80 MM; DESIGN RATING: 10 BAR; TEMPERATURE RATING: -40 TO 200 DEG C; CONNECTION: CENTER FLANGE; BODY MATERIAL: CI; FACE TO FACE LENGTH: 46 MM; OPERATED: LEVERLOCK; TRIM: STAINLESS STEEL; SOFTGOODS: NBR; APPLICATION: WATER; GRADE: 1.4409; SPECIFICATION: EN ISO 5211; STYLE: CENTERED DISC; SCHEDULE: EN 558 SERIES 20; SPECIAL FEATURES: NONE; MANUF P/N: Z011-A","PISTER, PAKER ,KLINGER MZANSI, SUPERPUMP,VALVES FOR AFTICA","BUTTERFLY; WAFER","80 MM","CI","10 BAR","STAINLESS STEEL","CENTER FLANGE","46 MM","`160 MM","LEVERLOCK","WATER","-40 TO 200 DEG C"]
["0657949","VALVE, BALL: VALVE SIZE: DN125; DESIGN RATING: PN16; TEMPERATURE RATING: 40 DEG C; CONNECTION: FLANGE; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 235 MM; OPERATED: ACTUATOR; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: PTFE; SPECIFICATION: ISO 9001; PORT TYPE: SCREW; APPLICATION: TURBINE; GRADE: 1.4301; TYPE: SHUT OFF; MODEL NO: FCKH; REFERENCE NO: 4423; WITH ROTORK ACTUATOR MODEL AB880M; PISTER.","WITH ROTORK ACTUATOR","BALL; SCREW; SHUT OFF","DN125","STAINLESS STEEL","PN16","STAINLESS STEEL","FLANGE","235 MM","210 MM","ACTUATOR","TURBINE","40 DEG C"]
["0657948","VALVE, BALL: VALVE SIZE: DN125; DESIGN RATING: PN100; TEMPERATURE RATING: 2-40 DEG C; CONNECTION: FLANGE; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 400 MM; OPERATED: ACTUATOR; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: PTFE; SPECIFICATION: ISO 9001; PORT TYPE: SCREW; APPLICATION: TURBINE; GRADE: 1.4301; TYPE: SHUT OFF; MODEL NO: FCKH; REFERENCE NO: 9423 486/13; COMPLETE WITH EXTENSION PART NUMBER 98651 P1 AND ROTORK ACTUATOR MODEL AB880M; PISTER.","PISTER, PAKER ,KLINGER MZANSI, SUPERPUMP,VALVES FOR AFTICA","BALL; SCREW; SHUT OFF","DN125","STAINLESS STEEL","PN100","STAINLESS STEEL","FLANGE","400 MM","250 MM","ACTUATOR","TURBINE","2-40 DEG C"]
["0657950","VALVE, BALL: VALVE SIZE: DN65; DESIGN RATING: PN100; TEMPERATURE RATING: 0-40 DEG C; CONNECTION: FLANGE; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 130 MM; OPERATED: ACTUATOR/LEVER; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: PTFE; SPECIFICATION: ISO 9001; PORT TYPE: SCREW; APPLICATION: TURBINE; GRADE: 1.4301; TYPE: SHUT OFF; MODEL NO: FCKH; REFERENCE NO: 9423 453/13; PISTER.","PISTER, PAKER ,KLINGER MZANSI, SUPERPUMP,VALVES FOR AFTICA","BALL; SCREW; SHUT OFF","DN65","STAINLESS STEEL","PN100","STAINLESS STEEL","FLANGE","130 MM","185 MM","ACTUATOR/LEVER","TURBINE","0-40 DEG C"]
["0655832","VALVE, BUTTERFLY: TYPE: WAFER; VALVE SIZE: 200 MM; DESIGN RATING: PN 16; TEMPERATURE RATING: -20 TO 200 DEG C; CONNECTION: FLANGE; BODY MATERIAL: CI; FACE TO FACE LENGTH: 60 MM; OPERATED: HANDWHEEL; TRIM: STAINLESS STEEL; SOFTGOODS: NBR; APPLICATION: VARIOUS; GRADE: 316; SPECIFICATION: ISO 9001; STYLE: 1 WAY; EBRO ARMATUREN","PISTER, PAKER ,KLINGER MZANSI, SUPERPUMP,VALVES FOR AFTICA","BUTTERFLY; WAFER","200 MM","CI","PN 16","STAINLESS STEEL","FLANGE","60 MM","295 MM","HANDWHEEL","VARIOUS","-20 TO 200 DEG C"]
["0655865","VALVE, BUTTERFLY: TYPE: WAFER; VALVE SIZE: 150 MM; DESIGN RATING: PN40; TEMPERATURE RATING: -20 TO 200 DEG F; CONNECTION: FLANGE; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 55 MM; OPERATED: HANDWHEEL; TRIM: STAINLESS STEEL; SOFTGOODS: PTFE; APPLICATION: VARIOUS; GRADE: 1.4408; STYLE: 1 WAY; EBRO ARMATUREN","PISTER, PAKER ,KLINGER MZANSI, SUPERPUMP,VALVES FOR AFTICA","BUTTERFLY; WAFER","150 MM","STAINLESS STEEL","PN40","STAINLESS STEEL","FLANGE","55 MM","285 MM","HANDWHEEL","VARIOUS","-20 TO 200 DEG F"]
["0620187","VALVE, BALL: VALVE SIZE: 1/2 IN; DESIGN RATING: 1 MPA; TEMPERATURE RATING: 100 DEG C; CONNECTION: MALE X FEMALE 1/2 IN; BODY MATERIAL: STEEL; FACE TO FACE LENGTH: 90 MM; OPERATED: LEVER; TYPE: SHUT OFF; OEM P/N: X13W-40P; YONP","PISTER, PARKER,HYDEC","BALL; SHUT OFF","1/2 IN","STEEL","1 MPA","STAINLESS STEEL, CARBON STEEL","MALE X FEMALE 1/2 IN","90 MM","N/A","LEVER","COOLING WATER, SERVICE WATER, HYDRAULIC OIL","100 DEG C"]
["0655834","VALVE, BUTTERFLY: TYPE: WAFER; VALVE SIZE: 600 MM; DESIGN RATING: PN 16; TEMPERATURE RATING: -20 TO 200 DEG C; CONNECTION: FLANGE; BODY MATERIAL: CI; FACE TO FACE LENGTH: 140 MM; OPERATED: HANDWHEEL; TRIM: STAINLESS STEEL; SOFTGOODS: EPDM 80 KTW; APPLICATION: VARIOUS; GRADE: 316; SPECIFICATION: ISO 9001; STYLE: 1 WAY; COMPLETE WITH ROTORK GEARBOX MODEL AB8600N/SP4; EBRO ARMATUREN","COMPLETE WITH ROTORK GEARBOX","BUTTERFLY; WAFER","600 MM","CI","PN 16","STAINLESS STEEL","FLANGE","140 MM","840 MM","HANDWHEEL","VARIOUS","-20 TO 200 DEG C"]
["0655831","VALVE, BUTTERFLY: TYPE: WAFER; VALVE SIZE: 300 MM; DESIGN RATING: PN 16; TEMPERATURE RATING: -20 TO 200 DEG C; CONNECTION: FLANGE; BODY MATERIAL: CI; FACE TO FACE LENGTH: 90 MM; OPERATED: HANDWHEEL; TRIM: STAINLESS STEEL; SOFTGOODS: NBR; APPLICATION: VARIOUS; GRADE: 316; SPECIFICATION: ISO 9001; STYLE: 1 WAY; EBRO ARMATUREN","PISTER, PAKER ,KLINGER MZANSI, SUPERPUMP,VALVES FOR AFTICA","BUTTERFLY; WAFER","300 MM","CI","PN 16","STAINLESS STEEL","FLANGE","90 MM","410 MM","HANDWHEEL","VARIOUS","-20 TO 200 DEG C"]
["0655867","VALVE, BUTTERFLY: TYPE: WAFER; VALVE SIZE: 300 MM; DESIGN RATING: PN25; TEMPERATURE RATING: -20 TO 200 DEG F; CONNECTION: FLANGE; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 77 MM; OPERATED: HANDWHEEL; TRIM: STAINLESS STEEL; SOFTGOODS: PTFE; APPLICATION: VARIOUS; GRADE: 1.4408; STYLE: 1 WAY; EBRO ARMATUREN","PISTER, PAKER ,KLINGER MZANSI, SUPERPUMP,VALVES FOR AFTICA","BUTTERFLY; WAFER","300 MM","STAINLESS STEEL","PN25","STAINLESS STEEL","FLANGE","77 MM","460 MM","HANDWHEEL","VARIOUS","-20 TO 200 DEG F"]
["0655833","VALVE, BUTTERFLY: TYPE: WAFER; VALVE SIZE: 150 MM; DESIGN RATING: PN 16; TEMPERATURE RATING: -20 TO 200 DEG C; CONNECTION: FLANGE; BODY MATERIAL: CI; FACE TO FACE LENGTH: 55 MM; OPERATED: LEVER; TRIM: STAINLESS STEEL; SOFTGOODS: NBR; APPLICATION: VARIOUS; GRADE: 316; SPECIFICATION: ISO 9001; STYLE: 1 WAY; EBRO ARMATUREN","PISTER, PAKER ,KLINGER MZANSI, SUPERPUMP,VALVES FOR AFTICA","BUTTERFLY; WAFER","150 MM","CI","PN 16","STAINLESS STEEL","FLANGE","55 MM","240 MM","LEVER","VARIOUS","-20 TO 200 DEG C"]
["0655866","VALVE, BUTTERFLY: TYPE: WAFER; VALVE SIZE: 200 MM; DESIGN RATING: PN40; TEMPERATURE RATING: -20 TO 200 DEG F; CONNECTION: FLANGE; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 60 MM; OPERATED: HANDWHEEL; TRIM: STAINLESS STEEL; SOFTGOODS: PTFE; APPLICATION: VARIOUS; GRADE: 1.4408; STYLE: 1 WAY; EBRO ARMATUREN","PISTER, PAKER ,KLINGER MZANSI, SUPERPUMP,VALVES FOR AFTICA","BUTTERFLY; WAFER","200 MM","STAINLESS STEEL","PN40","STAINLESS STEEL","FLANGE","60 MM","375 MM","HANDWHEEL","VARIOUS","-20 TO 200 DEG F"]
["0628206","VALVE, BUTTERFLY: TYPE: WAFER; VALVE SIZE: DN 100; DESIGN RATING: 10 BAR; TEMPERATURE RATING: -40 TO 200 DEG C; CONNECTION: CENTER FLANGE; BODY MATERIAL: CI; FACE TO FACE LENGTH: 52 MM; OPERATED: LEVERLOCK; TRIM: STAINLESS STEEL; SOFTGOODS: NBR; APPLICATION: WATER; GRADE: 1.4409; SPECIFICATION: EN ISO 5211; STYLE: CENTERED DISC; SCHEDULE: EN 558 SERIES 20; SPECIAL FEATURES: NONE; MANUF P/N: Z011-A; .","PISTER, PAKER ,KLINGER MZANSI, SUPERPUMP,VALVES FOR AFTICA","BUTTERFLY; WAFER","DN 100","CI","10 BAR","STAINLESS STEEL","CENTER FLANGE","52 MM","180 MM","LEVERLOCK","WATER","-40 TO 200 DEG C"]
["0637555","VALVE, CHECK: TYPE: NON RETURN; VALVE SIZE: G 3/4 IN; DESIGN RATING: 1 BAR; TEMPERATURE RATING: 0-100 DEG C; CONNECTION: THD; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 76 MM; OPERATED: AIR; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: STAINLESS STEEL; APPLICATION: COMPRESSOR; SPECIFICATION: V592; GRADE: 316; MANUF P/N: RHD20SOMD71; MODEL NO: WP6310; FOR USE ON JP SAUER AND SOHN COMPPRESSOR","PISTER, PAKER ,KLINGER MZANSI, SUPERPUMP,VALVES FOR AFTICA","CHECK; NON RETURN","G 3/4 IN","STAINLESS STEEL","1 BAR","STAINLESS STEEL","THD","76 MM","N/A","AIR","COMPRESSOR; JP SAUER AND SOHN COMPPRESSOR","0-100 DEG C"]
["0715945","VALVE, CHECK: TYPE: NON-RETURN; VALVE SIZE: 650 MM; DESIGN RATING: Y 0.35 AND VACUUM MPA; TEMPERATURE RATING: 200 DEG C; CONNECTION: BUTT-WELDED; BODY MATERIAL: STEEL ASTM A216-WCB; FACE TO FACE LENGTH: 1448 MM; OPERATED: AUTO; TRIM: STEEL; APPLICATION: CHECK VALVE LBS30AA501; SPECIFICATION: ANSI B16 34 CLASS 150; DRAWING NO: FB21EV650NFDA ITEM DEWRANCE; BLED STEAM CHECK VALVE, BODY: WBC, SEAT: CR13, DISK: CR18","Dewrance","CHECK; BODY; NON-RETURN","650 MM","STEEL ASTM A216-WCB","Y 0.35 AND VACUUM MPA","STEEL","BUTT-WELDED","1448 MM","N/A","AUTO","CHECK VALVE LBS30AA501","200 DEG C"]
["0655823","VALVE, CHECK: TYPE: PRESSURE; VALVE SIZE: DN400; DESIGN RATING: 16 BAR; TEMPERATURE RATING: -20 TO 200 DEG C; CONNECTION: FLANGED; BODY MATERIAL: CI; FACE TO FACE LENGTH: 480 MM; OPERATED: WATER; STYLE: 1 WAY; TRIM: 315E; SOFTGOODS: STAINLESS STEEL; APPLICATION: VARIOUS; SPECIFICATION: EN558/8; GRADE: GSC25; PERNOW","PERNOW, SUPERPUMP","CHECK; PRESSURE","DN400","CI","16 BAR","315E","FLANGED","480 MM","565 MM","WATER","VARIOUS","-20 TO 200 DEG C"]
["0623866","VALVE, SOLENOID: PIPE SIZE: PORT 7.5 MM; STYLE: 3/2; POTENTIAL: 24 VDC; DESIGN RATING: 350 BAR; CONNECTION: FLANGE; BODY MATERIAL: CI; OPERATED: PRESSURE; ENCLOSURE RATING: IP65; MEDIUM: OIL; POWER: 30 W; CURRENT: 1.25 A; APPLICATION: INTAKE EMERGENCY GATE HOIST; OEM P/N: M-3SED6UK13/350CG24N9K4, OEM: BOSCH REXROTH","Bosch; Rexroth","SOLENOID","PORT 7.5 MM","CI","350 BAR",null,"FLANGE",null,null,"PRESSURE","OIL; INTAKE EMERGENCY GATE HOIST"]
["0623874","VALVE, SOLENOID: PIPE SIZE: PORT 11 MM; STYLE: 4 WAY; POTENTIAL: 24 VDC; DESIGN RATING: 350 BAR; CONNECTION: FLANGE; BODY MATERIAL: CI; OPERATED: PRESSURE; ENCLOSURE RATING: IP65; MEDIUM: OIL; POWER: 40 W; CURRENT: 1.61 A; SOFTGOODS: SEALS NBR; APPLICATION: INTAKE HYDRAULIC POWER UNIT; SPECIFICATION: ISO 4401-05-04-0-05; OEM P/N: 4WE10C50/EG24N9K4/M, OEM: BOSCH REXROTH","Bosch; Rexroth","SOLENOID","PORT 11 MM","CI","350 BAR",null,"FLANGE",null,null,"PRESSURE","OIL; INTAKE HYDRAULIC POWER UNIT"]
["0726792","VALVE, SOLENOID: PIPE SIZE: 28 MM; STYLE: COAXIAL 3/2 WAY DIRECT ACTING; POTENTIAL: 230 VAC; DESIGN RATING: 100 BAR; CONNECTION: G3/4 IN FEMALE; BODY MATERIAL: BRASS; OPERATED: SOLENOID; ENCLOSURE RATING: IP65; MEDIUM: AIR; POWER: 0.4 W; CURRENT: 0.15 A; ORIFICE SIZE: 15 MM; SOFTGOODS: NBR ORING; APPLICATION: DRAIN VALVE; MANUF P/N: 039599; STAGE 3 DRAIN VALVE","Coax","SOLENOID","28 MM; 15 MM","BRASS","100 BAR",null,"G3/4 IN FEMALE",null,null,"SOLENOID","AIR; DRAIN VALVE"]
["0062540","VALVE, SOLENOID: POTENTIAL: 220 V; SUPPL P/N: S2155",null,"SOLENOID"]
["0668248","VALVE, SOLENOID: PIPE SIZE: 1-1/2 IN; STYLE: PLUNGER; POTENTIAL: 230 V; DESIGN RATING: 16 BAR; CONNECTION: THREADED; BODY MATERIAL: BRONZE; OPERATED: SOLENOID; ENCLOSURE RATING: NONE; MEDIUM: AIR; POWER: 16 W; CURRENT: 0.07 A; ORIFICE SIZE: 1-1/2 IN; APPLICATION: AUTO DRAIN",null,"SOLENOID","1-1/2 IN","BRONZE","16 BAR",null,"THREADED",null,null,"SOLENOID","AIR; AUTO DRAIN"]
["0617885","VALVE, SOLENOID: PIPE SIZE: 1/4 IN; STYLE: 2/1; POTENTIAL: 220 VDC; DESIGN RATING: 2 MPA; CONNECTION: IN; BODY MATERIAL: STEEL; OPERATED: SOLENOID TO OPEN, SPRING TO CLOSE; ENCLOSURE RATING: IP65; MEDIUM: GAS/LIQUID/OIL; POWER: 10 W; CURRENT: 22 A; DRAWING NO: M795-5E4971 REV 0; CAT NO: YS301GH27N9BC7",null,"SOLENOID","1/4 IN","STEEL","2 MPA",null,"IN",null,null,"SOLENOID TO OPEN, SPRING TO CLOSE","GAS/LIQUID/OIL"]
["0668261","VALVE, SOLENOID: PIPE SIZE: 1 IN; STYLE: PLUNGER; POTENTIAL: 230 V; DESIGN RATING: 33 BAR; CONNECTION: THREADED; BODY MATERIAL: BRONZE; OPERATED: SOLENOID; ENCLOSURE RATING: NONE; MEDIUM: AIR; POWER: 16 W; CURRENT: 0.07 A; ORIFICE SIZE: 1 IN; APPLICATION: AUTO DRAIN",null,"SOLENOID","1 IN","BRONZE","33 BAR",null,"THREADED",null,null,"SOLENOID","AIR; AUTO DRAIN"]
["0694573","VALVE, SOLENOID: PIPE SIZE: 1 IN; STYLE: 1/1; POTENTIAL: 24 VDC; DESIGN RATING: 10 BAR; CONNECTION: FNPT; BODY MATERIAL: STAINLESS STEEL; OPERATED: COIL SOLENOID VALVE; ENCLOSURE RATING: IP65; MEDIUM: DIESEL; ORIFICE SIZE: 15-25 MM; COIL: SINGLE; SOFTGOODS: O RING; APPLICATION: DIESEL; MODEL NO 2W-160-15, BOTH VALVE PORT; SIZE 1 IN",null,"SOLENOID","1 IN; 15-25 MM","STAINLESS STEEL","10 BAR",null,"FNPT",null,null,"COIL SOLENOID VALVE","DIESEL"]
["0659669","VALVE, RELIEF: VALVE SIZE: 1 IN; SET PRESSURE: 0.025-0.08 BAR; TEMPERATURE RATING: -10 TO 100 DEG C; CONNECTION: 1 X 1-1/2 IN; BODY MATERIAL: DIE-CAST AL; TRIM: OT 58 UNI 2012 BRS; FACE TO FACE LENGTH: 90 DEG; OPERATED: SPRING-LOADED; ORIFICE SIZE: 32 MM; SPECIFICATION: ISO 9001; APPLICATION: VARIOUS; STYLE: ONE WAY; SOFTGOODS: BUNA-N; DESIGN RATING: 6 BAR; PRESSURE RANGE: 0-6 BAR; OEM P/N: V/50; TARTARINI","REXROTH","RELIEF","1 IN; 32 MM","DIE-CAST AL","6 BAR; 0-6 BAR; 0.025-0.08 BAR","OT 58 UNI 2012 BRS","1 X 1-1/2 IN","90 DEG","N/A","SPRING-LOADED","VARIOUS","-10 TO 100 DEG C"]
["0623862","VALVE, CHECK: TYPE: FLOW CONTROL; VALVE SIZE: 1-1/4 IN; DESIGN RATING: 320 BAR; TEMPERATURE RATING: -20 TO 100 DEG C; CONNECTION: THD; BODY MATERIAL: STEEL; FACE TO FACE LENGTH: 134.5 MM; OPERATED: PRESSURE, 8 BAR; STYLE: 1 WAY; APPLICATION: SURGE CHAMBER HOIST; SPECIFICATION: EN 10083; OEM P/N: FT257/6 114 8 BAR","PISTER, PAKER ,KLINGER MZANSI, SUPERPUMP,VALVES FOR AFTICA","CHECK; FLOW CONTROL","1-1/4 IN","STEEL","320 BAR","HARDENED STEEL","THD","134.5 MM","N/A","PRESSURE, 8 BAR","SURGE CHAMBER HOIST","-20 TO 100 DEG C"]
["0637556","VALVE, CHECK: TYPE: NON RETURN; VALVE SIZE: 1-5/8 IN; DESIGN RATING: 10 BAR; TEMPERATURE RATING: 0-100 DEG C; CONNECTION: THD; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 118 MM; OPERATED: AIR; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: STAINLESS STEEL; APPLICATION: COMPRESSOR; SPECIFICATION: V592; GRADE: 42/L; MANUF P/N: 036471; MODEL NO: WP6310; FOR USE ON JP SAUER AND SOHN COMPRESSOR.","PERNOW, SUPERPUMP","CHECK; NON RETURN","1-5/8 IN","STAINLESS STEEL","10 BAR","STAINLESS STEEL","THD","118 MM","N/A","AIR","COMPRESSOR; JP SAUER AND SOHN COMPRESSOR","0-100 DEG C"]
["0637558","VALVE, CHECK: TYPE: NON RETURN; VALVE SIZE: DIN 50; DESIGN RATING: PN40; TEMPERATURE RATING: 0-100 DEG C; CONNECTION: THD FEMALE; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 150 MM; OPERATED: WATER; STYLE: 2 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: STAINLESS STEEL; APPLICATION: COMPRESSOR; SPECIFICATION: CE0062; GRADE: 1.4408; REFERENCE NO: M410; END ARMATUREN","PERNOW, SUPERPUMP","CHECK; NON RETURN","DIN 50","STAINLESS STEEL","PN40","STAINLESS STEEL","THD FEMALE","150 MM","N/A","WATER","COMPRESSOR","0-100 DEG C"]
["0628742","VALVE, CHECK: TYPE: NON RETURN; VALVE SIZE: DN 100; DESIGN RATING: PN40; TEMPERATURE RATING: -200 TO 550 DEG C; CONNECTION: FLANGE; BODY MATERIAL: CI 300; FACE TO FACE LENGTH: 60 MM; OPERATED: HAND; STYLE: 1 WAY; TRIM: STAINLESS STEEL; APPLICATION: VARIOUS; SPECIFICATION: (PED) 97/23/EC; GRADE: 1.4408; MANUF P/N: RK86A; WITH BODY CENTERING CAMS; FLOWSERVE","Flowserve Gestra","CHECK; NON RETURN","DN 100","CI 300","PN40","STAINLESS STEEL","FLANGE","60 MM","PCD: 190 mm Number of Holes: 8 holesHole Diameter: 22 mm (for M20 bolts)","HAND","VARIOUS","-200 TO 550 DEG C"]
["0637559","VALVE, CHECK: TYPE: NON RETURN; VALVE SIZE: DN 80; DESIGN RATING: PN100-160; TEMPERATURE RATING: 0-100 DEG C; CONNECTION: FLANGE; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 71 MM; OPERATED: WATER; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: STAINLESS STEEL; APPLICATION: COMPRESSOR; SPECIFICATION: CE 0525 05.14; GRADE: 1.4404; MANUF P/N: SR30.160","Gestra","CHECK; NON RETURN","DN 80","STAINLESS STEEL","PN100-160","STAINLESS STEEL","FLANGE","71 MM","Pitch Circle Diameter (PCD): 180 mmNumber of Bolt Holes: 8 holesBolt Hole Diameter: 26 mm (designed for M24 bolts)Flange Outside Diameter (OD): 230 mm","WATER","COMPRESSOR","0-100 DEG C"]
["0655829","VALVE, DIAPHRAGM: TYPE: WET PILOT ACTUATION; VALVE SIZE: 6 IN; DESIGN RATING: 250 PSI; TEMPERATURE RATING: -20 TO 200 DEG C; CONNECTION: FLANGED; BODY MATERIAL: CI; DIAPHRAGM MATERIAL: BUNA; FACE TO FACE LENGTH: 470 MM; OPERATED: PRESSURE; STYLE: 1 WAY; SOFTGOODS: BUNA; APPLICATION: SPRAY WATER; SPECIFICATION: ISO 9001; GRADE: 9YA4; MANUF P/N: DV506FS2","Tyco Fire Protection","DIAPHRAGM; WET PILOT ACTUATION","6 IN","CI; BUNA","250 PSI","BUNA","FLANGED","470 MM","Hole Diameter: 22 mm (for M20 bolts","PRESSURE","SPRAY WATER","-20 TO 200 DEG C"]
["0657954","VALVE, FLAPPER: TYPE: CHECK; BORE DIAMETER: DN65; CONNECTION: FLANGE; MATERIAL: STAINLESS STEEL; APPLICATION: TURBINE; SPECIFICATION: ISO 9001; MANUF P/N: 5N546CL; PRESSURE RATING: PN100; MATERIAL GRADE: 1.4408","VERVOVALVE,ORION VALVE","FLAPPER; CHECK","DN65","STAINLESS STEEL","PN100 (100 bar = 10 MPa / Approx. 1450 PSI or Class 600)","GX5CrNiMo19-11-2 / Cast 316 Stainless Steel / CF8M","FLANGE","Face-to-Face Dimension: 46 mm (1.81 inches)","Flange Outer Diameter (OD): 205 mmBolt Circle Diameter (PCD): 145 mmBolt Hole Quantity: 8 holesBolt Hole Diameter: 26 mm (Uses M24 size bolts)","Valve Type: Check Valve / Non-Return Valve (Flapper / Swing Type). It operates automatically using line pressure to allow unidirectional fluid flow and prevent dangerous backflow or water hammer. [1, 2, 3, 4, 5]","TURBINE","100°C: 100.0 bar"]
["0657955","VALVE, FLAPPER: TYPE: CHECK; BORE DIAMETER: DN80; CONNECTION: FLANGE; MATERIAL: STAINLESS STEEL; APPLICATION: TURBINE; SPECIFICATION: ISO 9001; MANUF P/N: 4N602CL; PRESSURE RATING: PN160; MATERIAL GRADE: 1.4408","Velan Inc, Atwood & Morrill (Trillium Flow Technologies),Sempell (Emerson)","FLAPPER; CHECK","DN80 (80mm / approx. 3-inch)","STAINLESS STEEL","PN160 (160 Bar / 16 MPa / approx. 2320 PSI)","Stainless Steel Grade 1.4408 (GX5CrNiMo19-11-2)","FLANGE","46 mm","Bolt Circle Diameter (PCD): 145 mm","IN LINE FLOW CONTROLLED","TURBINE","-196°C up to +400°C"]
["0620393","VALVE, GATE: VALVE SIZE: 100 MM; TYPE: ISOLATING; CONNECTION: FLANGE; FACE TO FACE LENGTH: 300 MM; BODY MATERIAL: SCS13; TRIM: SS GR 304; OPERATED: HANDWHEEL; STEM DESIGN: RISING; STYLE: 1 WAY; TEMPERATURE RATING: 20 K; APPLICATION: AIR COOLER; DESIGN RATING: JIS 20 K","KITZ Corporation , Shoritsu (Japan) , Bestway Valve (China) , J-Valves Fluid Equipment (China)","GATE; ISOLATING","100 MM","SCS13","JIS 20 K","SS GR 304; RISING","FLANGE","300 MM","Pitch Circle Diameter (PCD): 185 mmNumber of Bolt Holes: 8 holesBolt Hole Diameter: 23 mmRecommended Bolt Size: M20","HANDWHEEL","AIR COOLER","20 K"]
["0620394","VALVE, GATE: VALVE SIZE: 1-1/2 IN; TYPE: ISOLATING; CONNECTION: FLANGE; FACE TO FACE LENGTH: 160 MM; BODY MATERIAL: A105; TRIM: 13CR; OPERATED: HANDWHEEL; STEM DESIGN: RISING; STYLE: 1 WAY; TEMPERATURE RATING: 840 DEG F; APPLICATION: OIL LEVEL; DESIGN RATING: JIS 10K; .","KITZ Corporation (Japan) , Toyo Valve (Japan) , Hitachi Valves , Velan or Neway","GATE; ISOLATING","1-1/2 IN","A105","JIS 10K","13CR; RISING","FLANGE","160 MM","Pitch Circle Diameter (PCD): 105 mmNumber of Bolt Holes: 4 holesBolt Hole Diameter: 19 mm Recommended Bolt Size: M16","HANDWHEEL","OIL LEVEL","840 DEG F"]
["0620397","VALVE, GATE: VALVE SIZE: 200 MM; TYPE: ISOLATING; CONNECTION: FLANGE; FACE TO FACE LENGTH: 450 MM; BODY MATERIAL: SCS13; TRIM: SS GR 304; OPERATED: CHAIN, HANDWHEEL; STEM DESIGN: RISING; STYLE: 1 WAY; TEMPERATURE RATING: 20K DEG F; APPLICATION: AIR COOLER; DESIGN RATING: JIS 20 K","KITZ Corporation (Japan): , Tozen Corporation , Shoritsu Seisakusho","GATE; ISOLATING","200 MM","SCS13","JIS 20 K","SS GR 304; RISING","FLANGE","450 MM","Pitch Circle Diameter (PCD): 305 mm Number of Bolt Holes: 12 holesBolt Hole Diameter: 25 mm Recommended Nominal Bolt Size: M22","CHAIN, HANDWHEEL","AIR COOLER","20K DEG F"]
["0620398","VALVE, GATE: VALVE SIZE: 200 MM; TYPE: ISOLATING; DESIGN PRESSURE: JIS 20 K; DESIGN TEMPERATURE: 20 K; CONNECTION: FLANGE; FACE TO FACE LENGTH: 450 MM; BODY MATERIAL: SCS13; TRIM: SS GR 304; OPERATED: HANDWHEEL; STEM DESIGN: RISING; STYLE: 1 WAY; TEMPERATURE RATING: 20K DEG F; APPLICATION: OIL COOLER; DESIGN RATING: JIS 20K K","KITZ Corporation , Toyo Valve Co., Ltd , Toa Valve Engineering Inc","GATE; ISOLATING","200 MM","SCS13","JIS 20K K; JIS 20 K","SS GR 304; RISING","FLANGE","450 MM","PCD (Pitch Circle Diameter): 305 mm Number of Bolt Holes: 12 holesBolt Hole Diameter: 25 mm (Uses M22 bolts)Flange Outer Diameter (OD): 350 mm","HANDWHEEL","OIL COOLER","20K DEG F; 20 K"]
["0620391","VALVE, GATE: VALVE SIZE: 250 MM; TYPE: ISOLATING; DESIGN PRESSURE: 2-2.8 MPA; DESIGN TEMPERATURE: 220-350 DEG C; CONNECTION: FLANGE; FACE TO FACE LENGTH: 455 MM; BODY MATERIAL: STAINLESS STEEL; TRIM: HF; OPERATED: ACTUATOR; STEM DESIGN: NON RISING; STYLE: 1 WAY; TEMPERATURE RATING: 20 K; PORT TYPE: STANDARD; APPLICATION: TURBINE; SPECIFICATION: ISO 9001; SPECIAL FEATURES: NONE; GRADE: 304; DESIGN RATING: JIS 20K","KITZ Corporation , Velan Inc. , Kubota Corporation","GATE; ISOLATING; STANDARD","250 MM","STAINLESS STEEL","JIS 20K; 2-2.8 MPA","HF; NON RISING","FLANGE","455 MM","Pitch Circle Diameter (PCD): 380 mm (The center-to-center diameter of the bolt circle)Number of Bolt Holes: 12 holesBolt Hole Diameter: 27 mm (Designed to fit metric M24 flange bolts)","ACTUATOR","TURBINE","20 K; 220-350 DEG C"]
["0655828","VALVE, DIAPHRAGM: TYPE: WET PILOT ACTUATION; VALVE SIZE: 4 IN; DESIGN RATING: 250 PSI; TEMPERATURE RATING: -20 TO 200 DEG C; CONNECTION: FLANGED; BODY MATERIAL: CI; DIAPHRAGM MATERIAL: BUNA; FACE TO FACE LENGTH: 400 MM; OPERATED: PRESSURE; STYLE: 1 WAY; SOFTGOODS: BUNA; APPLICATION: SPRAY WATER; SPECIFICATION: ISO 9001; GRADE: 9YA4; MANUF P/N: DV504FS2","Tyco Fire Protection Products, a brand under Johnson Controls","DIAPHRAGM; WET PILOT ACTUATION","4 IN","CI; BUNA","250 PSI","BUNA","FLANGED","400 MM","No of holes :8","PRESSURE","SPRAY WATER","-20 TO 200 DEG C"]
["0637405","VALVE, CHECK: TYPE: RIGHT ANGLE; VALVE SIZE: 3 IN; DESIGN RATING: 21 MPA; TEMPERATURE RATING: -15 TO 75 DEG C; CONNECTION: BOLTED; BODY MATERIAL: STL ALLOY; FACE TO FACE LENGTH: 72.5 X 87 MM; OPERATED: SPRING; MODEL NO: C2G-805-S3","Tokyo Keiki Inc. / TOKIMEC","CHECK; RIGHT ANGLE","3 IN","STL ALLOY","21 MPA","Alloy Steel.","BOLTED","72.5 X 87 MM","Bolt Hole Diameter: 27 mm (Designed to fit metric M24 flange bolts","SPRING","STANDARD INDUSTRIAL USE","-15 TO 75 DEG C"]
["0721178","VALVE, CHECK: TYPE: TL34; VALVE SIZE: 3 IN; DESIGN RATING: 2 BAR; TEMPERATURE RATING: -40-100 DEG C; CONNECTION: DN 80, 3 IN PIPE; BODY MATERIAL: ALSI7MG0.65T685HBS; FACE TO FACE LENGTH: 1.00 M; OPERATED: 250 VDC SUPPLY; TL34 CONSERVATOR SHUTTER VALVE; MAXIMUM SWITCHING, VOLTAGE 250 VDC; BODY MATERIAL: ALSI7MG0.6ST685 HBS; 3 IN; SIZE: DN80; SERGI (FRANCE)","SERGI","CHECK; TL34","3 IN","ALSI7MG0.65T685HBS; ALSI7MG0.6ST685 HBS","2 BAR","STAINLESS STEEL","DN 80, 3 IN PIPE","1.00 M","160 MM","250 VDC SUPPLY","TRANSFORMER OIL ","-40-100 DEG C"]
["0731175","VALVE, CHECK: TYPE: TL34; VALVE SIZE: DN80; DESIGN RATING: 2 BAR; TEMPERATURE RATING: -40 to 100 DEG C; CONNECTION: SIZE 0 GLAND; BODY MATERIAL: CAST IRON; FACE TO FACE LENGTH: 210.5 MM; OPERATED: 220VDC","KLINGER,SUPERPUMP","CHECK; TL34","DN80","CAST IRON","2 BAR","STAINLESS STEEL","SIZE 0 GLAND","210.5 MM","160 MM","220VDC","TRANSFORMER OIL SYSTEMS, COMPRESSORS","-40 to 100 DEG C"]
["0635725","VALVE, CHECK: TYPE: WAFER; VALVE SIZE: DN65; DESIGN RATING: 20 BAR; TEMPERATURE RATING: 0-120 DEG C; CONNECTION: FLANGE; BODY MATERIAL: GGG40; FACE TO FACE LENGTH: 46 MM; OPERATED: FLOW; STYLE: 1 WAY; TRIM: STAINLESS STEEL; SOFTGOODS: EPDM; APPLICATION: CHILLER; GRADE: 1.4401; MANUF P/N: 915S25/1/E; DUAL WAFER","KLINGER,SUPERPUMP","CHECK; WAFER","DN65","GGG40","20 BAR","STAINLESS STEEL","FLANGE","46 MM","N/A","FLOW","CHILLER","0-120 DEG C"]
["0623867","VALVE, CHECK: TYPE: SUBPLATE; VALVE SIZE: NS10; DESIGN RATING: 350 BAR; TEMPERATURE RATING: -20 TO 80 DEG C; CONNECTION: FLANGE; BODY MATERIAL: CI; FACE TO FACE LENGTH: 50 MM; OPERATED: OIL PRESSURE; STYLE: 1/1; SOFTGOODS: FKM; APPLICATION: INTAKE HYDRAULIC POWER UNIT; SPECIFICATION: DIN 51524; OEM P/N: Z1S10B05-2-41/F, OEM: BOSCH REXROTH","Bosch; Rexroth","CHECK; SUBPLATE","NS10","CI","350 BAR","HARDENED STEEL, SPRING STEEL","FLANGE","50 MM","N/A","OIL PRESSURE","INTAKE HYDRAULIC POWER UNIT","-20 TO 80 DEG C"]
["0623870","VALVE, CHECK: TYPE: TWIN THROTTLE; VALVE SIZE: NS6; DESIGN RATING: 315 BAR; TEMPERATURE RATING: -20 TO 80 DEG C; CONNECTION: FLANGE; BODY MATERIAL: CI; FACE TO FACE LENGTH: 40 MM; OPERATED: OIL PRESSURE; SOFTGOODS: SEALS FKM; APPLICATION: INTAKE HYDRAULIC POWER UNIT; SPECIFICATION: DIN 51524; OEM P/N: Z2FS6-2-44/2QV, OEM: BOSCH REXROTH; .","Bosch; Rexroth","CHECK; TWIN THROTTLE","NS6","CI","315 BAR","HARDENED STEEL","FLANGE","40 MM","N/A","OIL PRESSURE","INTAKE HYDRAULIC POWER UNIT","-20 TO 80 DEG C"]
["0620183","VALVE, GLOBE: VALVE SIZE: 1/2 IN; DESIGN PRESSURE: 2.0 MPA; DESIGN TEMPERATURE: <100 DEG C; FACE TO FACE LENGTH: 150 MM; OPERATED: HANDWHEEL; CONNECTION: FLANGED; BODY MATERIAL: F304; TRIM: SS GR 304/STL; GRADE: ASTM A182 F304; SOFTGOODS: NEOPRENE; STEM DESIGN: RISING SPINDLE; STYLE: DIRECTIONAL; APPLICATION: DRAIN AIR/OIL COOLER; SPECIFICATION: ISO9001; TYPE: SHUT OFF; DESIGN RATING: JIS 20K; S AND S VALVE","VALVE FOR AFRICA ,SUPERPUMP, KLINGER MZANSI","GLOBE; SHUT OFF","1/2 IN","F304","JIS 20K; 2.0 MPA","SS GR 304/STL; RISING SPINDLE","FLANGED","150 MM","70 MM","HANDWHEEL","DRAIN AIR/OIL COOLER","<100 DEG C"]
["0064665","VALVE, GLOBE: VALVE SIZE: 15 MM; OPERATED: MANUAL; CONNECTION: SW; BODY MATERIAL: CS; DESIGN RATING: 600 LB; MANUF P/N: SASSWJ0015BR","VALVE FOR AFRICA ,SUPERPUMP, KLINGER MZANSI","GLOBE","15 MM","CS","600 LB","STELLITE, STAINLESS STEEL","SW","110 - 140 MM","N/A","MANUAL","WATER, OIL, AIR","–20°C to 100°C"]
["0620408","VALVE, GLOBE: VALVE SIZE: 2 IN; FACE TO FACE LENGTH: 200 MM; OPERATED: HANDWHEEL; CONNECTION: FLANGE; BODY MATERIAL: A105; TRIM: 13CR; STEM DESIGN: RISING; STYLE: 1 WAY; APPLICATION: DRAIN; TYPE: ISOLATING; DESIGN RATING: JIS 10K; TEMPERATURE RATING: 840 DEG F","PAKER, SUPERPUMP , HYDRAULICS, PISTER","GLOBE; ISOLATING","2 IN","A105","JIS 10K","13CR; RISING","FLANGE","200 MM","120 MM","HANDWHEEL","DRAIN","840 DEG F"]
["0620407","VALVE, GLOBE: VALVE SIZE: 50 MM; FACE TO FACE LENGTH: 200 MM; OPERATED: HANDWHEEL; CONNECTION: FLANGE; BODY MATERIAL: SCS13; TRIM: SS GR 304; STEM DESIGN: RISING; STYLE: 1 WAY; APPLICATION: DRAIN; TYPE: ISOLATING; DESIGN RATING: JIS 20K; TEMPERATURE RATING: 20K","PAKER, SUPERPUMP , HYDRAULICS, PISTER","GLOBE; ISOLATING","50 MM","SCS13","JIS 20K","SS GR 304; RISING","FLANGE","200 MM","120 MM","HANDWHEEL","DRAIN","20K"]
["0620181","VALVE, GLOBE: VALVE SIZE: 1/2 IN; DESIGN PRESSURE: 1 TO 1.2 MPA; DESIGN TEMPERATURE: 220 TO 300 DEG C; FACE TO FACE LENGTH: 105 MM; OPERATED: HANDWHEEL; CONNECTION: FLANGED; BODY MATERIAL: A105; TRIM: STL 13CR; GRADE: ASTM A105; SOFTGOODS: NEOPRENE; STEM DESIGN: RISING SPINDLE; STYLE: DIRECTIONAL; APPLICATION: OIL DRAIN; SPECIFICATION: ISO 9001; TYPE: SHUT OFF; DESIGN RATING: JIS 10K; TEMPERATURE RATING: 100 DEG F; OEM P/N: SC-F10K-15A; S AND S VALVE","PAKER, SUPERPUMP , HYDRAULICS, PISTER,","GLOBE; SHUT OFF","1/2 IN","A105","JIS 10K; 1 TO 1.2 MPA","STL 13CR; RISING SPINDLE","FLANGED","105 MM","70 MM","HANDWHEEL","OIL DRAIN","100 DEG F; 220 TO 300 DEG C"]
["0620186","VALVE, GLOBE: VALVE SIZE: 1 IN; DESIGN PRESSURE: 1 TO 1.2 MPA; DESIGN TEMPERATURE: 220 TO 300 DEG C; FACE TO FACE LENGTH: 125 MM; OPERATED: HANDWHEEL; CONNECTION: FLANGED; BODY MATERIAL: A105; TRIM: 13CR/STL; GRADE: ASTM A105; SOFTGOODS: NEOPRENE; STEM DESIGN: RISING SPINDLE; STYLE: DIRECTIONAL; APPLICATION: DRAIN; SPECIFICATION: ISO 9001; TYPE: SHUT OFF; DESIGN RATING: JIS 10K; TEMPERATURE RATING: 840 DEG F; OEM P/N: SC-F10K-25A; S AND S VALVE","PAKER, SUPERPUMP , HYDRAULICS, PISTER","GLOBE; SHUT OFF","1 IN","A105","JIS 10K; 1 TO 1.2 MPA","13CR/STL; RISING SPINDLE","FLANGED","125 MM","90 MM","HANDWHEEL","DRAIN","840 DEG F; 220 TO 300 DEG C"]
["0623904","VALVE, RELIEF: VALVE SIZE: NS40; SET PRESSURE: ADJUSTABLE; TEMPERATURE RATING: -20 TO 80 DEG C; CONNECTION: FLANGE; BODY MATERIAL: CAST IRON; TRIM: CAST IRON; FACE TO FACE LENGTH: 100 MM; OPERATED: OIL PRESSURE; ORIFICE SIZE: DIA 1.18 MM; SPECIFICATION: DIN 24340; APPLICATION: DRAFT TUBE GATE HOIST; STYLE: 2 WAY; DESIGN RATING: 420 BAR; PRESSURE RANGE: 0-420 BAR; OEM P/N: LFA40H2-71/F, OEM: BOSCH REXROTH; TO BE SUPPLIED WITH VALVE CARTRIDGE LC 40 A05E7X R900937996","Bosch; Rexroth","RELIEF","NS40; DIA 1.18 MM","CAST IRON","420 BAR; 0-420 BAR; ADJUSTABLE","CAST IRON","FLANGE","100 MM","N/A","OIL PRESSURE","DRAFT TUBE GATE HOIST","-20 TO 80 DEG C"]
["0623903","VALVE, RELIEF: VALVE SIZE: NS16; SET PRESSURE: ADJUSTABLE; TEMPERATURE RATING: -20 TO 80 DEG C; CONNECTION: FLANGE; BODY MATERIAL: CAST IRON; TRIM: CAST IRON; FACE TO FACE LENGTH: 35 MM; OPERATED: OIL PRESSURE; ORIFICE SIZE: DIA 0.669 MM; SPECIFICATION: DIN 24340; APPLICATION: DRAFT TUBE GATE HOIST; STYLE: 2 WAY; DESIGN RATING: 420 BAR; PRESSURE RANGE: 0-420 BAR; OEM P/N: LFA16H2-71/F, OEM: BOSCH REXROTH; TO BE SUPPLIED WITH VALVE CARTRIDGE LC 16 A05E7X R900912566","Bosch; Rexroth","RELIEF","NS16; DIA 0.669 MM","CAST IRON","420 BAR; 0-420 BAR; ADJUSTABLE","CAST IRON","FLANGE","35 MM","N/A","OIL PRESSURE","DRAFT TUBE GATE HOIST","-20 TO 80 DEG C"]
["0655228","VALVE, RELIEF: VALVE SIZE: G1/2 IN; SET PRESSURE: 365 KPA; TEMPERATURE RATING: -10 TO 220 DEG C; CONNECTION: G1/2 IN; BODY MATERIAL: 1.4104 (430); TRIM: METAL; FACE TO FACE LENGTH: 46 MM; OPERATED: PRESSURE; ORIFICE SIZE: 10 MM; SPECIFICATION: DIN ISO 228-1; APPLICATION: VARIOUS; GRADE: 1.4104; STYLE: 1 WAY; SOFTGOODS: 1.4404; DESIGN RATING: PN160-400; PRESSURE RANGE: 180-365 BAR; MANUF P/N: 4373.2602; REFERENCE NO: D0 10-D/G 0.5 F 0.35; .","REXROTH","RELIEF","G1/2 IN; 10 MM","1.4104 (430)","PN160-400; 180-365 BAR; 365 KPA","METAL","G1/2 IN","46 MM","N/A","PRESSURE","VARIOUS","-10 TO 220 DEG C"]
["0639776","VALVE, RELIEF: VALVE SIZE: G1/2 IN; SET PRESSURE: 3 BAR; TEMPERATURE RATING: 0-20 DEG C; CONNECTION: G1/2 IN; BODY MATERIAL: SS GR 316L; TRIM: SS GR 316L; FACE TO FACE LENGTH: 90 DEG; OPERATED: PRESSURE; ORIFICE SIZE: 1/2 IN; APPLICATION: VARIOUS; GRADE: 1.4404; STYLE: 1 WAY; SOFTGOODS: STAINLESS STEEL; DESIGN RATING: INLET PN250; OUTLET PN160; PRESSURE RANGE: 0-250 BAR; REFERENCE NO: 4374.3144","REXROTH","RELIEF","G1/2 IN; 1/2 IN","SS GR 316L","INLET PN250; 0-250 BAR; 3 BAR","SS GR 316L","G1/2 IN","90 DEG","N/A","PRESSURE","VARIOUS","0-20 DEG C"]
["0620399","VALVE, GATE: VALVE SIZE: 250 MM; TYPE: ISOLATING; CONNECTION: FLANGE; FACE TO FACE LENGTH: 450 MM; BODY MATERIAL: SCS13; TRIM: SS GR 304; OPERATED: CHAIN, HANDWHEEL; STEM DESIGN: RISING; STYLE: 1 WAY; TEMPERATURE RATING: 20K DEG F; APPLICATION: COOLER; DESIGN RATING: JIS 20K; .","PAKER, SUPERPUMP , HYDRAULICS, PISTER","GATE; ISOLATING","250 MM","SCS13","JIS 20K","SS GR 304; RISING","FLANGE","450 MM","370 MM","CHAIN, HANDWHEEL","COOLER","20K DEG F"]
["0620395","VALVE, GATE: VALVE SIZE: 300 MM; TYPE: ISOLATING; CONNECTION: FLANGE; FACE TO FACE LENGTH: 500 MM; BODY MATERIAL: SCS13; TRIM: SS GR 304; OPERATED: CHAIN, HANDWHEEL; STEM DESIGN: RISING; STYLE: 1 WAY; TEMPERATURE RATING: 20K DEG F; APPLICATION: AIR COOLER; DESIGN RATING: JIS 20K; .","PAKER, SUPERPUMP , HYDRAULICS, PISTER","GATE; ISOLATING","300 MM","SCS13","JIS 20K","SS GR 304; RISING","FLANGE","500 MM","430 MM","CHAIN, HANDWHEEL","AIR COOLER","20K DEG F"]
["0620396","VALVE, GATE: VALVE SIZE: 300 MM; TYPE: ISOLATING; DESIGN PRESSURE: JIS 20 K; DESIGN TEMPERATURE: 20 K; CONNECTION: FLANGE; FACE TO FACE LENGTH: 500 MM; BODY MATERIAL: SCS13; TRIM: SS GR 304; OPERATED: HANDWHEEL; STEM DESIGN: RISING; STYLE: 1 WAY; TEMPERATURE RATING: 20K DEG F; APPLICATION: OIL COOLER; DESIGN RATING: JIS 20 K","ENERGY VALVES,KLINGER VALVES, FLUID HAUS,SUPERPUMP","GATE; ISOLATING","300 MM","SCS13","JIS 20 K","SS GR 304; RISING","FLANGE","500 MM","430 MM","HANDWHEEL","OIL COOLER","20K DEG F; 20 K"]
["0620392","VALVE, GATE: VALVE SIZE: 50 MM; TYPE: ISOLATING; CONNECTION: FLANGE; FACE TO FACE LENGTH: 213 MM; BODY MATERIAL: SCS13; TRIM: SS GR 304; OPERATED: HANDWHEEL; STEM DESIGN: RISING; STYLE: 1 WAY; TEMPERATURE RATING: 20K K; APPLICATION: UPPER OIL COOLER; DESIGN RATING: JIS 20K K","ENERGY VALVES,KLINGER VALVES, FLUID HAUS,SUPERPUMP","GATE; ISOLATING","50 MM","SCS13","JIS 20K K","SS GR 304; RISING","FLANGE","213 MM",null,"HANDWHEEL","UPPER OIL COOLER","20K K"]
["0628697","VALVE, RELIEF: VALVE SIZE: 3/4 IN; SET PRESSURE: 47.2 BAR; TEMPERATURE RATING: -10 TO 100 DEG C; CONNECTION: THREADED FEMALE; BODY MATERIAL: BRASS; TRIM: BRASS; FACE TO FACE LENGTH: 118 MM; OPERATED: PRESSURE; ORIFICE SIZE: 10 MM; SPECIFICATION: ISO 4126-1; APPLICATION: VARIOUS; STYLE: 1 WAY; SOFTGOODS: BRASS; DESIGN RATING: 150 BAR; PRESSURE RANGE: 42-25 BAR; MANUF P/N: H10N11787","REXROTH","RELIEF","3/4 IN; 10 MM","BRASS","150 BAR; 42-25 BAR; 47.2 BAR","BRASS","THREADED FEMALE","118 MM","N/A","PRESSURE","VARIOUS","-10 TO 100 DEG C"]
["0637561","VALVE, RELIEF: VALVE SIZE: DN 3/4 X 1 IN; SET PRESSURE: 53 BAR; TEMPERATURE RATING: -20 TO 200 DEG C; CONNECTION: THD; BODY MATERIAL: BRASS; TRIM: BRASS; FACE TO FACE LENGTH: L SHAPE; OPERATED: AIR; ORIFICE SIZE: 1/2 IN; SPECIFICATION: CE 0035 2011; APPLICATION: COMPRESSOR; GRADE: G14/S; STYLE: 1 WAY; SOFTGOODS: BRASS; MANUF P/N: CW614N","REXROTH","RELIEF","DN 3/4 X 1 IN; 1/2 IN","BRASS","53 BAR","BRASS","THD","L SHAPE","N/A","AIR","COMPRESSOR","-20 TO 200 DEG C"]
["0655227","VALVE, RELIEF: VALVE SIZE: DN 1 X 1-1/4 IN; SET PRESSURE: 8 BAR; TEMPERATURE RATING: -20 TO 200 DEG C; CONNECTION: THD; BODY MATERIAL: BRZ; TRIM: BRZ; FACE TO FACE LENGTH: L SHAPE; OPERATED: PRESSURE; ORIFICE SIZE: 1/2 IN; SPECIFICATION: CE0036 2017; APPLICATION: COMPRESSOR; GRADE: G20/S; STYLE: 1 WAY; SOFTGOODS: BRZ; MANUF P/N: 017450016","REXROTH","RELIEF","DN 1 X 1-1/4 IN; 1/2 IN","BRZ","8 BAR","BRZ","THD","L SHAPE","N/A","PRESSURE","COMPRESSOR","-20 TO 200 DEG C"]
["0623863","VALVE, RELIEF: VALVE SIZE: NS10; SET PRESSURE: ADJUSTABLE; TEMPERATURE RATING: 100 DEG C; CONNECTION: FLANGE; BODY MATERIAL: CAST IRON; TRIM: CAST IRON; FACE TO FACE LENGTH: 30 MM; OPERATED: PILOT; ORIFICE SIZE: ADJUSTABLE; SPECIFICATION: 97/23/EC; APPLICATION: SURGE CHAMBER HOIST; STYLE: 1 WAY; SOFTGOODS: O-RING; DESIGN RATING: 200 BAR; PRESSURE RANGE: 0-200 BAR; OEM P/N: DBW10B2-52/300-6EG24N9K4, OEM: BOSCH REXROTH; WITH BUILT-ON DIRECTIONAL VALVE","Bosch; Rexroth","RELIEF","NS10; ADJUSTABLE","CAST IRON","200 BAR; 0-200 BAR; ADJUSTABLE","CAST IRON","FLANGE","30 MM","N/A","PILOT","SURGE CHAMBER HOIST","100 DEG C"]
["0644952","VALVE, RELIEF: VALVE SIZE: 30 MM; SET PRESSURE: 100 BAR; TEMPERATURE RATING: -30 TO 80 DEG C; CONNECTION: SUBPLATE; BODY MATERIAL: STEEL; TRIM: METAL; FACE TO FACE LENGTH: 80 MM; OPERATED: PRESSURE; ORIFICE SIZE: 15 MM; SPECIFICATION: ISO 9001; APPLICATION: VARIOUS; GRADE: 913000149; STYLE: 1 WAY; SOFTGOODS: NBR; DESIGN RATING: 25-400 BAR; PRESSURE RANGE: 0-350 BAR; MANUF P/N: R900423712; MODEL NO: DBDS 30 P1A/100","REXROTH","RELIEF","30 MM; 15 MM","STEEL","25-400 BAR; 0-350 BAR; 100 BAR","METAL","SUBPLATE","80 MM","N/A","PRESSURE","VARIOUS","-30 TO 80 DEG C"]
["0068148","VALVE, RELIEF: VALVE SIZE: 50 MM; SET PRESSURE: 35 KPA; CONNECTION: THD; BODY MATERIAL: STL; TRIM: BRASS; OPERATED: SPRING; PRESSURE RANGE: 2-20 LB; REFERENCE NO: MD0014; SAFETY; TYPE 616-2; TYPE: HLP","REXROTH","RELIEF; HLP","50 MM","STL","2-20 LB; 35 KPA","BRASS","THD","N/A","N/A","SPRING","AIR, WATER, OIL, NON-CORROSIVE GASES","–20°C to ~120°C"]
["0619974","VALVE, RELIEF: VALVE SIZE: 1/2 IN; SET PRESSURE: 1.5 MPA; TEMPERATURE RATING: 120 DEG C; CONNECTION: BSP SCREW; BODY MATERIAL: STEEL; TRIM: STEEL; FACE TO FACE LENGTH: T-TYPE; OPERATED: PRESSURE; APPLICATION: PRESSURE REDUCER; DESIGN RATING: 1.5 MPA; PRESSURE RANGE: 1.3-1.5 MPA; REFERENCE NO: ESV-903M","REXROTH","RELIEF","1/2 IN","STEEL","1.5 MPA; 1.3-1.5 MPA","STEEL","BSP SCREW","T-TYPE","N/A","PRESSURE","PRESSURE REDUCER","120 DEG C"]
["0623857","VALVE, RELIEF: VALVE SIZE: 1 IN; SET PRESSURE: 94 BAR; TEMPERATURE RATING: 100 DEG C; CONNECTION: FLANGE; BODY MATERIAL: CAST IRON; TRIM: CAST IRON; FACE TO FACE LENGTH: 26 MM; OPERATED: PILOT; ORIFICE SIZE: ADJUSTABLE; SPECIFICATION: ANSI B16.10; APPLICATION: SURGE CHAMBER HOIST; STYLE: 3/2; SOFTGOODS: O-RING; DESIGN RATING: 315 BAR; PRESSURE RANGE: 0-315 BAR; OEM P/N: DB20-2-52/315, OEM: BOSCH REXROTH","Bosch; Rexroth","RELIEF","1 IN; ADJUSTABLE","CAST IRON","315 BAR; 0-315 BAR; 94 BAR","CAST IRON","FLANGE","26 MM","N/A","PILOT","SURGE CHAMBER HOIST","100 DEG C"]
["0660516","VALVE, PILOT: VALVE STYLE: 1 WAY; VALVE SIZE: 6 MM; MATERIAL: STL; OEM P/N: GPFX730094P0001, OEM: ABB POWER GENERATION (PTY) LTD; MODEL NO: HECPS-3S/5S; 220-250 VDC; FOR USE ON GEN CIRCUIT BREAKER; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",null,"PILOT","6 MM","STL",{"$nulls":6},"GEN CIRCUIT BREAKER"]
["0659664","VALVE, RELIEF: VALVE SIZE: 8 MM; SET PRESSURE: 11 BAR; TEMPERATURE RATING: -20 TO 200 DEG C; CONNECTION: R1/2 IN; BODY MATERIAL: BRASS; TRIM: STEEL; FACE TO FACE LENGTH: CASCADE; OPERATED: PRESSURE; ORIFICE SIZE: 6 MM; SPECIFICATION: EN 4126-1; APPLICATION: VARIOUS; STYLE: ONE WAY; SOFTGOODS: BRASS; DESIGN RATING: 15 BAR; PRESSURE RANGE: 0.73-15 BAR; OEM P/N: 03/16-08711; BOGE COMPRESSED AIR SYSTEMS","REXROTH,VOITH","RELIEF","8 MM; 6 MM","BRASS","15 BAR; 0.73-15 BAR; 11 BAR","STEEL","R1/2 IN","CASCADE","N/A","PRESSURE","VARIOUS","-20 TO 200 DEG C"]
["0637560","VALVE, RELIEF: VALVE SIZE: 1 IN; SET PRESSURE: 88 BAR; TEMPERATURE RATING: 0-50 DEG C; CONNECTION: G1 IN-BSPP; BODY MATERIAL: STAINLESS STEEL; TRIM: STAINLESS STEEL; FACE TO FACE LENGTH: L SHAPE; OPERATED: AIR; ORIFICE SIZE: 1 IN; SPECIFICATION: GL1238640; APPLICATION: COMPRESSOR; GRADE: 316; STYLE: 1 WAY; SOFTGOODS: STAINLESS STEEL; DESIGN RATING: 88 BAR G; PRESSURE RANGE: IN PN 250; OUT PN 40; MANUF P/N: M33H03X00V56V66J23H01","REXROTH,VOITH","RELIEF","1 IN","STAINLESS STEEL","88 BAR G; IN PN 250; 88 BAR","STAINLESS STEEL","G1 IN-BSPP","L SHAPE","N/A","AIR","COMPRESSOR","0-50 DEG C"]
["0617883","VALVE, RELIEF: VALVE SIZE: 1/2 IN; SET PRESSURE: 2.1 MPA; TEMPERATURE RATING: 220 DEG C; CONNECTION: 1/2 IN-BSP; BODY MATERIAL: STEEL; TRIM: VARIOUS; FACE TO FACE LENGTH: 110 MM; OPERATED: PRESSURE; APPLICATION: AIR LINES; DESIGN RATING: 2.1 MPA; PRESSURE RANGE: 0-2.1 MPA; DRAWING NO: M705-5A7443A REV 0","REXROTH,VOITH","RELIEF","1/2 IN","STEEL","2.1 MPA; 0-2.1 MPA","VARIOUS","1/2 IN-BSP","110 MM","N/A","PRESSURE","AIR LINES","220 DEG C"]
["0637562","VALVE, RELIEF: VALVE SIZE: 1/2 IN; SET PRESSURE: 3 BAR; TEMPERATURE RATING: 0-20 DEG C; CONNECTION: THD 1/2 IN; BODY MATERIAL: STAINLESS STEEL; TRIM: STAINLESS STEEL; FACE TO FACE LENGTH: L SHAPE; OPERATED: AIR; ORIFICE SIZE: 1 IN; SPECIFICATION: 14/980; APPLICATION: COMPRESSOR; GRADE: 316; STYLE: 1 WAY; SOFTGOODS: STAINLESS STEEL; DESIGN RATING: 3 BAR; PRESSURE RANGE: IN PN 250; OUT PN 160; MANUF P/N: M33H03X00V54V65; .","REXROTH,VOITH","RELIEF","1/2 IN; 1 IN","STAINLESS STEEL","3 BAR; IN PN 250","STAINLESS STEEL","THD 1/2 IN","L SHAPE","N/A","AIR","COMPRESSOR","0-20 DEG C"]
["0644950","VALVE, RELIEF: VALVE SIZE: 10 MM; SET PRESSURE: 130 BAR; TEMPERATURE RATING: -30 TO 80 DEG C; CONNECTION: THREADED; BODY MATERIAL: STEEL; TRIM: METAL; FACE TO FACE LENGTH: 80 MM; OPERATED: PRESSURE; ORIFICE SIZE: 5 MM; SPECIFICATION: ISO 9001; APPLICATION: VARIOUS; GRADE: 913000149; STYLE: 1 WAY; SOFTGOODS: NBR; DESIGN RATING: 25-400 BAR; PRESSURE RANGE: 0-630 BAR; MANUF P/N: R900778044; MODEL NO: DBDS 10 G19/130E","REXROTH,VOITH","RELIEF","10 MM; 5 MM","STEEL","25-400 BAR; 0-630 BAR; 130 BAR","METAL","THREADED","80 MM","N/A","PRESSURE","VARIOUS","-30 TO 80 DEG C"]
["0644949","VALVE, RELIEF: VALVE SIZE: 10 MM; SET PRESSURE: 65 BAR; TEMPERATURE RATING: -30 TO 80 DEG C; CONNECTION: THREADED; BODY MATERIAL: STEEL; TRIM: METAL; FACE TO FACE LENGTH: 80 MM; OPERATED: PRESSURE; ORIFICE SIZE: 5 MM; SPECIFICATION: ISO 9001; APPLICATION: VARIOUS; GRADE: 913000149; STYLE: 1 WAY; SOFTGOODS: NBR; DESIGN RATING: 25-400 BAR; PRESSURE RANGE: 0-630 BAR; MANUF P/N: R901260712; MODEL NO: DBDS 10 G19/65E","REXROTH,VOITH","RELIEF","10 MM; 5 MM","STEEL","25-400 BAR; 0-630 BAR; 65 BAR","METAL","THREADED","80 MM","N/A","PRESSURE","VARIOUS","-30 TO 80 DEG C"]
["0644951","VALVE, RELIEF: VALVE SIZE: 30 MM; SET PRESSURE: 130 BAR; TEMPERATURE RATING: -30 TO 80 DEG C; CONNECTION: SUBPLATE; BODY MATERIAL: STEEL; TRIM: METAL; FACE TO FACE LENGTH: 80 MM; OPERATED: PRESSURE; ORIFICE SIZE: 15 MM; SPECIFICATION: ISO 9001; APPLICATION: VARIOUS; GRADE: 913000149; STYLE: 1 WAY; SOFTGOODS: NBR; DESIGN RATING: 25-400 BAR; PRESSURE RANGE: 0-350 BAR; MANUF P/N: R901341824; MODEL NO: DBDS 30 G1A/130E","REXROTH,VOITH","RELIEF","30 MM; 15 MM","STEEL","25-400 BAR; 0-350 BAR; 130 BAR","METAL","SUBPLATE","80 MM","N/A","PRESSURE","VARIOUS","-30 TO 80 DEG C"]
["0644953","VALVE, RELIEF: VALVE SIZE: 20 MM; SET PRESSURE: 100 BAR; TEMPERATURE RATING: -30 TO 80 DEG C; CONNECTION: SUBPLATE; BODY MATERIAL: STEEL; TRIM: METAL; FACE TO FACE LENGTH: NIL; OPERATED: PRESSURE; ORIFICE SIZE: 10 MM; SPECIFICATION: ISO 9001; APPLICATION: VARIOUS; GRADE: 913000149; STYLE: 1 WAY; SOFTGOODS: NBR; DESIGN RATING: 25-400 BAR; PRESSURE RANGE: 10-350 BAR; MANUF P/N: R900597283; MODEL NO: DR 20-5-52/100YM","REXROTH, VOITH","RELIEF","20 MM; 10 MM","STEEL","25-400 BAR; 10-350 BAR; 100 BAR","METAL","SUBPLATE","NIL","N/A","PRESSURE","VARIOUS","-30 TO 80 DEG C"]
["0637402","VALVE, RELIEF: VALVE SIZE: 3 IN; SET PRESSURE: 25 MPA; TEMPERATURE RATING: -15 TO 75 DEG C; CONNECTION: THD; BODY MATERIAL: STL CAST; TRIM: BONNET CS; FACE TO FACE LENGTH: 150.5 X 90 MM; OPERATED: PILOT; MODEL NO: BT-03-32","REXROTH, SIZANANI VALVES","RELIEF","3 IN","STL CAST","25 MPA","BONNET CS","THD","150.5 X 90 MM","N/A","PILOT","VARIOUS","-15 TO 75 DEG C"]
["0783932","VALVE, BUTTERFLY: TYPE: VALVE BUTTERFLY; VALVE SIZE: DN 80 MM; DESIGN RATING: PN16 BAR; TEMPERATURE RATING: 95; CONNECTION: RUBBER SEALING; BODY MATERIAL: GG-25; FACE TO FACE LENGTH: 46 MM; OPERATED: ACTUATOR","SUPERPUMP, KLINGER MZANSI","BUTTERFLY; VALVE BUTTERFLY","DN 80 MM","GG-25","PN16 BAR","STAINLESSTEEL","RUBBER SEALING","46 MM","N/A","ACTUATOR","WATER",95]

{"sheet":"Palmiet Pumped Storage","index":13,"n_rows":98,"n_cols":14,"rows_kept":98}
["Material","Original Description","OEM / Manufacturer","Valve Type","Size","Body Material","Class / Rating","Trim / Internals","End Connection","Face-to-Face","Drilling / PCD","Operation","Medium / Service","Medium Temperature"]
["0043039","HEAD, CYLINDER: TYPE: 1ST STG VALVE; SUPPL P/N: 4656; ITEM 23 POS 230, SIZE 128MM X 128 MM X 20 MM;USED ON THE SULZER BURCKHART COMPRESSOR TYPE C4N2F","C4N2F","1ST STG VALVE",{"$nulls":8},"THE SULZER BURCKHART COMPRESSOR TYPE C4N2F"]
["0062308","VALVE, RELIEF: VALVE SIZE: 24 X 12 MM; SET PRESSURE: 14.5 KGF/CM; CONNECTION: NPT X FNPT; BODY MATERIAL: BRASS; REFERENCE NO: M096-84176222/23P10; SAFETY; POP; TYPE RCX-SO; SEAT DIA. 12MM","RCX-SO","RELIEF","24 X 12 MM","BRASS","14.5 KGF/CM",null,"NPT X FNPT"]
["0062309","VALVE, SOLENOID: PIPE SIZE: 1/4 IN; STYLE: 3 WAY; POTENTIAL: 220 VDC; DESIGN RATING: 35 KGF/CM; CONNECTION: FNPT; BODY MATERIAL: BRASS; MEDIUM: AIR/GAS/OIL/WATER; POWER: 9.7 W; ORIFICE SIZE: 3/64 IN; DRAWING NO: M096-8417222/23P8 REV 1; CAT NO: T8262D19; REFERENCE NO: 364202; 8321A2; GENERAL PURPOSE ENCLOSURE","ASCO","SOLENOID","1/4 IN; 3/64 IN","BRASS","35 KGF/CM",null,"FNPT",{"$nulls":3},"AIR/GAS/OIL/WATER"]
["0062311","VALVE, SOLENOID: PIPE SIZE: 3/8 IN; STYLE: 2 WAY; POTENTIAL: 220 VDC; DESIGN RATING: 0.7/14 KGF/CM; CONNECTION: FNPT; BODY MATERIAL: BRASS; MEDIUM: AIR/GAS/OIL/WATER; POWER: 9.7 W; ORIFICE SIZE: 9/32 IN; REFERENCE NO: 364201; 8263D19; GENERAL PURPOSE ENCLOSURE","ASCO","SOLENOID","3/8 IN; 9/32 IN","BRASS","0.7/14 KGF/CM",null,"FNPT",{"$nulls":3},"AIR/GAS/OIL/WATER"]
["0062312","VALVE, SOLENOID: PIPE SIZE: 10 MM; STYLE: 4/2 WAY; POTENTIAL: 250 VAC; DESIGN RATING: 315 BAR; CONNECTION: COMPRESSION; BODY MATERIAL: STEEL; OPERATED: DC SOLENOID; ENCLOSURE RATING: IP54; MEDIUM: AIR/LIQUID; POWER: 36 W; MANUF P/N: S10G51G0230615MV; CAT NO: 52051.9000; HERION DIRECTIONAL CONTROL VALVE - PRESSURE TEST CERTIFICATES TO BE SUPPLIED ON DELIVERY","Herion","SOLENOID","10 MM","STEEL","315 BAR",null,"COMPRESSION",null,null,"DC SOLENOID","AIR/LIQUID"]
["0177857","VALVE: TYPE: CONTROL; VALVE SIZE: 38 MM; CONNECTION: FLANGE; OPERATED: AIR; BODY MATERIAL: CS; STYLE: BOLTED BONNET; TRIM: DISC STL","Fisher","CONTROL","38 MM","CS",null,"DISC STL","FLANGE",null,null,"AIR"]
["0664392","VALVE: TYPE: PLUG; VALVE SIZE: DN 150; DESIGN RATING: PN64; TEMPERATURE RATING: 0-100 DEG C; CONNECTION: FLANGE DN150/PN64; OPERATED: HYDRAULIC; BODY MATERIAL: CS; SUPPL P/N: 2612; VOITH RUNNER RELIEF VALVE; ORDER NUMBER: 5/5044; TYPE: 2.41-48660 PRESSURE TEST CERTIFICATES TO BE SUPPLIED WITH VALVE; VALVE DRAWING WITH BILL OF MATERIALS/PARTS LIST TO BE SUPPLIED","Voith","PLUG; 2.41-48660 PRESSURE TEST CERTIFICATES TO BE SUPPLIED WITH VALVE","DN 150","CS","PN64",null,"FLANGE DN150/PN64",null,null,"HYDRAULIC",null,"0-100 DEG C"]
["0688401","VALVE, RELIEF: VALVE SIZE: 100 X 125 MM; SET PRESSURE: 25-2400 KPA G; TEMPERATURE RATING: -4 TO -230 DEG C; CONNECTION: FLANGE; BODY MATERIAL: CS; TRIM: DISC ST/ST; FACE TO FACE LENGTH: 187/165 MM; OPERATED: SPRING; ORIFICE SIZE: SQ 2027 MM; SPECIFICATION: BS 6759-3:1984; APPLICATION: BFPT LUB OIL BYPASS PRESSURE; SOFTGOODS: GASKET INORGANIC FIBRE WITH NITRILE BINDER; DESIGN RATING: 2.4 MPA; REFERENCE NO: 693; SC81S503 & SC71S09; INLET FACE TO OUTLET CENTRE 187 MM; OUTLET FACE TO INLET CENTRE 16 5 MM; CAST STEEL SINGLE SPRING HIGH LIFT SAFETY RELIEF VALVE; INLET FLANGE DN 100 BS10-H; OUTLET FLANGE DN125 BS10-F; SPRING OPERATED TO OPEN WHEN SET SPRING TENSION IS OVERCOME BY SYSTEM PRESSURE; SEAT RING ST/ST; SPRING STEEL; ALL OTHER DIMENSIONS TO BS 6759-3:1984; VALVE TO BE SUPPLIED WITH A SET PRESSURE CERTIFICATE; FLANGES TO BE COVERED OR PLUGGED TO PREVENT FOREIGN MATERIAL FROM ENTERING, AND PROTECTED FROM THE ELEMENTS WITH A SUITABLE CORROSION INHIBITOR; A TECHNICAL EVALUATION NEEDS TO BE DONE PRIOR TO ORDER PLACEMENT; THE FOLLOWING DOCUMENTS ARE REQUIRED FOR THE TECHNICAL EVALUATION (1) GENERAL VALVE ASSEMBLY DRAWING (2) VALVE BROCHURE/INFORMATION; SIGNED ASSEMBLY DRAWING BY THE SUPPLIER WILL SERVE AS PROOF FOR THE CORRECT ITEM TO BE SUPPLIED; NO QUALITY CHECK WILL BE DONE WITHOUT A TECHNICAL EVALUATION BEING DONE DURING THE TENDERING STAGE; FOR VALVES THAT ARE TO BE REFURBISHED, A REFURBISHED SOW MUST BE SUBMITTED BY TURBINE ENGINEERING; THIS SOW MUST BE ISSUED WITH THE TENDERS; NO REPAIRS WILL BE PERMITTED OR ACCEPTED WITHOUT THE ENGINEERING SOW BEING SUPPLIED AND ADHERED TO","LESER","RELIEF","100 X 125 MM; SQ 2027 MM","CS","2.4 MPA; 25-2400 KPA G","DISC ST/ST","FLANGE","187/165 MM",null,"SPRING","BFPT LUB OIL BYPASS PRESSURE","-4 TO -230 DEG C"]
["0714976","VALVE, PLUG: VALVE SIZE: 80; DESIGN RATING: PN40; TEMPERATURE RATING: -10 TO 100 CELSIUS; CONNECTION: THREADED CONNECTION (G1/2); BODY MATERIAL: CARBON STEEL; FACE TO FACE LENGTH: 155 MM; OPERATED: HYDRAULIC; SOFTGOODS: O-RING RUBBER 85X3 / O-RING RUBBER 102X3 / MANTEL-RING TFMA 90X88X7.3 / NUT-RINGB12X24X10 / SCRAPER-RING B12X22; CONFIGURATION: FLANGE; APPLICATION: COMPRESSED AIR; TYPE: BLOWDOWN; MANUF P/N: 2.49-581","SchuF Group","PLUG; BLOWDOWN","80","CARBON STEEL","PN40",null,"THREADED CONNECTION (G1/2)","155 MM",null,"HYDRAULIC","COMPRESSED AIR","-10 TO 100 CELSIUS"]
["0728675","VALVE, RELIEF: VALVE SIZE: 1 IN; SET PRESSURE: 64 BAR; TEMPERATURE RATING: -30 TO 100 DEG C; CONNECTION: G1 IN; BODY MATERIAL: FREE CUTTING STEEL; TRIM: FREE CUTTING STEEL; FACE TO FACE LENGTH: 115 MM; OPERATED: PILOT; APPLICATION: HYDRAULIC PUMP; STYLE: SPOOL TYPE; SOFTGOODS: NBR O-RINGS; DESIGN RATING: 125 BAR; PRESSURE RANGE: 5 -125 BAR; MANUF P/N: DB16P; MODEL NO: DB16P-01-C-N-190V","Yuken","RELIEF","1 IN","FREE CUTTING STEEL","125 BAR; 5 -125 BAR; 64 BAR","FREE CUTTING STEEL","G1 IN","115 MM",null,"PILOT","HYDRAULIC PUMP","-30 TO 100 DEG C"]
["0731743","VALVE, CHECK: TYPE: SWING DISK NRV; VALVE SIZE: 3 IN; DESIGN RATING: PN 16; TEMPERATURE RATING: 0 TO 100 DEG C; CONNECTION: FLANGED; BODY MATERIAL: ASTM 216; FACE TO FACE LENGTH: 66 MM; OPERATED: SPRING ACTUATED; STYLE: WAFER TYPE SWING CHECK; SPECIFICATION: FM,UL,CUL APPROVED; MANUF P/N: V03312; PRESSURE TEST AND MATERIAL TEST CERTIFICATES TO BE SUPPLIED UPON DELIVERY OF THE VALVES.","SWING","CHECK; SWING DISK NRV","3 IN","ASTM 216","PN 16",null,"FLANGED","66 MM",null,"SPRING ACTUATED",null,"0 TO 100 DEG C"]
["0731847","VALVE, RELIEF: VALVE SIZE: G 1/4 IN; SET PRESSURE: 11 BAR; TEMPERATURE RATING: -20 TO 200 DEG C; CONNECTION: THREADED; BODY MATERIAL: BRASS; TRIM: BRASS - STAINLESS STEEL; FACE TO FACE LENGTH: 65 MM; OPERATED: SPRING LOADED - MECHANICALLY; ORIFICE SIZE: 38.47 MM2; SPECIFICATION: ASME VIII DIV. 1; APPLICATION: COMPRESSED AIR; STYLE: FREE DISCHARGE - D7; SOFTGOODS: N.B.R.(STD) -10 / + 100 °C; DESIGN RATING: PN60; PRESSURE RANGE: 8 - 12 BAR; MANUF P/N: D7CW614N; SAFETY VALVE TO BE SET AT 11 BAR (COLD SET PRESSURE). SAFETY VALVE TO BE TAGGED AND LED SEALED. INFORMATION ON TAG SHOULD CONTAIN:VALVE SERIAL NUMBER, SET PRESSURE, TEST DATE AND DUE DATE. DUE DATE SHOULD BE 3 YEARS FROM TEST DATE. VALVE. TEST REPORT TO BE SUPPLIED ALONG WITH VALVE.TEST REPORT TO DETAIL TO CORRESPOND WITH VALVE INFO","Nuova General Instruments S.r.l.","RELIEF","G 1/4 IN; 38.47 MM2","BRASS","PN60; 8 - 12 BAR; 11 BAR","BRASS - STAINLESS STEEL","THREADED","65 MM",null,"SPRING LOADED - MECHANICALLY","COMPRESSED AIR","-20 TO 200 DEG C"]
["0767444","VALVE: TYPE: PRESSURE RELIEF; VALVE SIZE: 1/4 IN; DESIGN RATING: 0.3-10 BAR; TEMPERATURE RATING: -34 TO 65 DEG C; CONNECTION: G1/4 IN; OPERATED: 10BAR; BODY MATERIAL: ZINC ALLOY; MANUF P/N: V07-200NGMG; V07; NORGREN, MINIATURE PORTED","Norgren","PRESSURE RELIEF","1/4 IN","ZINC ALLOY","0.3-10 BAR",null,"G1/4 IN",null,null,"10BAR",null,"-34 TO 65 DEG C"]
["0028911","BELT: TYPE: VALVE; FIG NO: 2396C.S. SA1253 B77; REFERENCE NO: 44411-006B; FOR 3 INCH HOPKINSON VALVE; USED FOR SOOTBLOWER REHEAT SECTION; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","No further information available","VALVE"]
["0068400","VALVE, CHECK: VALVE SIZE: 20 MM; DESIGN RATING: 20 BAR; TEMPERATURE RATING: 9 BAR AT 180 DEG C; CONNECTION: THD FEMALE; BODY MATERIAL: BRZ; STYLE: THD CAP; TRIM: DISC BRZ; MODEL NO: SS3501/M; REFERENCE NO: ES701; TYPE LIFT; IN LINE; CKI; FOR USE ON BOILER; MATERIAL AND TEST CERTIFICATES, TO DIN 50049/3.1B, ARE TO BE SUPPLIED ON DELIVERY","LIFT","CHECK","20 MM","BRZ","20 BAR","DISC BRZ","THD FEMALE",{"$nulls":3},"BOILER","9 BAR AT 180 DEG C"]
["0068955","VALVE, CHECK: TYPE: SWING; VALVE SIZE: 280 MM; TEMPERATURE RATING: 200 DEG C; CONNECTION: BW; STYLE: BOLTED CAP; TRIM: DISC/SEAT 13CRS; GRADE: WCB; WEIGHT ASSISTED; BODY 37.5BAR; SEAT 25BAR","NEWAY","CHECK; SWING","280 MM",null,null,"DISC/SEAT 13CRS","BW",{"$nulls":4},"200 DEG C"]
["0515330","MASK: TYPE: DUST; DIMENSIONS: 207 MM; PROTECTION FOR WHICH DESIGNED: DUST; SPECIAL FEATURES: WITH VALVE; SUPPL P/N: FFP2; PPE","No further information available","DUST"]
["0751707","VALVE, GATE: VALVE SIZE: DN150 MM; TYPE: WEDGE; DESIGN PRESSURE: 16 BAR; DESIGN TEMPERATURE: +/- 80 DEG C; CONNECTION: FLANGE; FACE TO FACE LENGTH: 210 MM; BODY MATERIAL: CAST IRON; TRIM: WEDGE; OPERATED: HANDWHEEL; STEM DESIGN: RISING SPINDLE; TEMPERATURE RATING: +/- 80 DEG C; APPLICATION: COOLING TOWERS ISOLATION; DESIGN RATING: 16 BAR; OPERATED: HANDWHEEL RISING SPINDLE; DESIGN RATING: 16 BAR; DRILING: SANS1123 – TABLE 600","AVK","GATE; WEDGE","DN150 MM","CAST IRON","16 BAR","WEDGE; RISING SPINDLE","FLANGE","210 MM","SANS1123 – TABLE 600","HANDWHEEL; HANDWHEEL RISING SPINDLE","COOLING TOWERS ISOLATION","+/- 80 DEG C"]
["0751861","VALVE, CHECK: TYPE: WAFER; VALVE SIZE: 400 MM; DESIGN RATING: 1600 KPA; TEMPERATURE RATING: 0 TO 100 DEG C; CONNECTION: FLANGE; BODY MATERIAL: CF8M; FACE TO FACE LENGTH: 108 MM; OPERATED: SPRING ACTUATED; STYLE: WAFER; TRIM: CF8M; SOFTGOODS: NITRILE; OEM P/N: 16DMZ; MODEL NO: 16DMZ; FIG NO: 16DMZ, SERIAL NO:821186, PRESSURE TEST AND MATERIAL TEST CERTIFICATES TO BE SUPPLIED WITH VALVES.","NEWAY","CHECK; WAFER","400 MM","CF8M","1600 KPA","CF8M","FLANGE","108 MM",null,"SPRING ACTUATED",null,"0 TO 100 DEG C"]
["0762729","VALVE, RELIEF: VALVE SIZE: 172 X 90 MM; SET PRESSURE: 8 PSI; TEMPERATURE RATING: -30 TO -120 DEG C; CONNECTION: FLANGE; BODY MATERIAL: WEATHERPROOF AND TRANSFORMER OIL RESISTANT ALUMINIUM; TRIM: SPRING STEEL EN 10270-1; OPERATED: SPRING; SPECIFICATION: IEC 60947-5-1 AC-15 / DC-13; APPLICATION: PALMIET GEN TRANSFORMER; STYLE: SIGNAL PIN INDICATOR; SOFTGOODS: MOUNTING GASKET 200 X 178.5 X 4.25 MM","MESSKO","RELIEF","172 X 90 MM","WEATHERPROOF AND TRANSFORMER OIL RESISTANT ALUMINIUM","8 PSI","SPRING STEEL EN 10270-1","FLANGE",null,null,"SPRING","PALMIET GEN TRANSFORMER","-30 TO -120 DEG C"]
["0778355","PROTECTOR: TYPE: SHUTTER VALVE; DIMENSIONS: 80 MM; MATERIAL: ALUMINIUM; MANUF P/N: 1RDR100800; POWER SUPPLY 220V AC OR DC, BREAKING CAPACITY 2A, RATED CURRENT 0.5A FOR 10.000 MANOEUVERS","COMEM","SHUTTER VALVE",null,"ALUMINIUM"]
["0717459","VALVE: TYPE: HYDRAULIC; VALVE SIZE: 0.5 MM; DESIGN RATING: 65 BAR; TEMPERATURE RATING: -10 TO 100 BAR; FACE TO FACE LENGTH: 286 MM; CONNECTION: BSP 1/4 IN / 1/2 BSP IN; OPERATED: HYDRAULIC; BODY MATERIAL: CARBON STEEL-UPPER AND MIDDLE BLOCK BRASS -; STYLE: UPPER BLOCK COMPRESSION SPRING - MIDDLE BLOCK HYDRAULIC -LOWER BLOCK WATER; TRIM: COMPRESSION SPRING 35X45X100 - WIRE 5MM - COILS 8; SOFTGOODS: 8X2NBR70 ORINGS -32X3NBR ORINGS -20X3BNR70 ORINGS; SPECIAL FEATURES: HYDRAULIC TELL TALE HOLES,PILOTED WITH WATER; MANUF P/N: 3/5010 2.41-32489; SQUARE TYPE O RING,TAPPERED BOTTOM THICKNESS 4MM PAPER 5.3 - 6.3 MM ID 11 MM OD 21 MM TAPERED BOTTOM 21.6 PAPERED TOP 11 MM, MANTEL RING TFMI 16X18X3/19X2.5 MM O-RING HYDRAULIC MIDDLE SECTION M10 MOUTING HOLES","No further information available","HYDRAULIC","0.5 MM","CARBON STEEL-UPPER AND MIDDLE BLOCK BRASS -","65 BAR","COMPRESSION SPRING 35X45X100 - WIRE 5MM - COILS 8","BSP 1/4 IN / 1/2 BSP IN","286 MM",null,"HYDRAULIC",null,"-10 TO 100 BAR"]
["0041764","VALVE: TYPE: UNLOADING; FOR CONDENSATE B/DOWN","No further information available","UNLOADING"]
["0041832","VALVE: TYPE: COMPRESSOR; VALVE SIZE: 280 MM; OPERATED: PRESSURE; BODY MATERIAL: STL; TRIM: DISC SS; 1ST STAGE CONCENTRIC","No further information available","COMPRESSOR","280 MM","STL",null,"DISC SS",{"$nulls":3},"PRESSURE"]
["0041833","VALVE: TYPE: COMPRESSOR; VALVE SIZE: 175 MM; OPERATED: PRESSURE; BODY MATERIAL: STL; TRIM: DISC SS; 2ND STAGE CONCENTRIC","No further information available","COMPRESSOR","175 MM","STL",null,"DISC SS",{"$nulls":3},"PRESSURE"]
["0041834","VALVE: TYPE: COMPRESSOR; VALVE SIZE: 95 MM; OPERATED: PRESSURE; BODY MATERIAL: STL; TRIM: DISC SS; 3RD STAGE CONCENTRIC","No further information available","COMPRESSOR","95 MM","STL",null,"DISC SS",{"$nulls":3},"PRESSURE"]
["0050087","VALVE, SOLENOID: PIPE SIZE: 15 MM; STYLE: 2 WAY; CONNECTION: FNPT; BODY MATERIAL: STEEL; MEDIUM: OIL; SUPPL P/N: 2VA2/43A-002/1 T6; DISTRIBUTION BLOCK","No further information available","SOLENOID","15 MM","STEEL",null,null,"FNPT",{"$nulls":3},"OIL"]
["0050088","VALVE, SOLENOID: PIPE SIZE: 12 MM; STYLE: 4 WAY; CONNECTION: FNPT; BODY MATERIAL: STEEL; MEDIUM: OIL; SUPPL P/N: ZVA 2/22A-002/1 T6; DISTRIBUTION BLOCK 1 WAY","No further information available","SOLENOID","12 MM","STEEL",null,null,"FNPT",{"$nulls":3},"OIL"]
["0050089","VALVE, SOLENOID: PIPE SIZE: 12 MM; STYLE: 3 WAY; CONNECTION: FNPT; BODY MATERIAL: STEEL; MEDIUM: OIL; SUPPL P/N: ZA2-66A-002/1 T6; DISTRIBUTION BLOCK","No further information available","SOLENOID","12 MM","STEEL",null,null,"FNPT",{"$nulls":3},"OIL"]
["0050090","VALVE, SOLENOID: PIPE SIZE: 15 MM; STYLE: 2 WAY; CONNECTION: FNPT; BODY MATERIAL: STEEL; MEDIUM: OIL; SUPPL P/N: ZVA2-44A-002-1 T6; DISTRIBUTION BLOCK","No further information available","SOLENOID","15 MM","STEEL",null,null,"FNPT",{"$nulls":3},"OIL"]
["0050092","VALVE, SOLENOID: PIPE SIZE: 12 MM; STYLE: 4 WAY; CONNECTION: FNPT; BODY MATERIAL: STEEL; MEDIUM: OIL; SUPPL P/N: ZVA2-88A-002-1 T6; DISTRIBUTION BLOCK","No further information available","SOLENOID","12 MM","STEEL",null,null,"FNPT",{"$nulls":3},"OIL"]
["0069346","VALVE, RELIEF: VALVE SIZE: 30 X 15 MM; SET PRESSURE: 64 BAR; CONNECTION: NPT X FNPT; BODY MATERIAL: STL; TRIM: DISC SS; SPRING STL; OPERATED: PRESSURE, SPRING; FULL STROKE SPRING TYPE SAFETY; GEBR LESER TYPE 561; D/G 0.8; BEST NUMBER: 615875/5003","SAFETY; Leser","RELIEF","30 X 15 MM","STL","64 BAR","DISC SS","NPT X FNPT",null,null,"PRESSURE, SPRING"]
["0069359","VALVE, PLUG: VALVE SIZE: 15 MM; CONNECTION: FNPT; BODY MATERIAL: BRASS; OPERATED: HANDWHEEL; STYLE: THD BONNET; TRIM: BONNET/PLUG BRS; TYPE: SHUT OFF; DRAWING NO: M096-84176222/23P9 REV 1; REFERENCE NO: NBV1003GX; PACKLESS; RIGHT - LEFT OPEN INDICATION; 3/8 INCH; MP 30KG/CM","DATA NOT AVAILABLE","PLUG; SHUT OFF","15 MM","BRASS",null,"BONNET/PLUG BRS","FNPT",null,null,"HANDWHEEL"]
["0142398","CLUTCH: TYPE: SOLENOID VALVE; BORE: 19 MM; DRAWING NO: HATM 302903 P001 REV 1; 110 VOLT; SIZE OD 85.7 X WD 38.4MM; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","No further information available","SOLENOID VALVE"]
["0655128","VALVE, BUTTERFLY: TYPE: STRAINER; VALVE SIZE: DN50; DESIGN RATING: 16 BAR; TEMPERATURE RATING: -10 TO 110 DEG C; CONNECTION: MALE COUPLING; BODY MATERIAL: CI; FACE TO FACE LENGTH: 45 MM; OPERATED: ACTUATOR; TRIM: DISC SS; SHAFT SS;BODY SEAT EPDM; SOFTGOODS: RUBBER; SUPPL P/N: IBF3SS","AVK","BUTTERFLY; STRAINER","DN50","CI","16 BAR","DISC SS","MALE COUPLING","45 MM",null,"ACTUATOR",null,"-10 TO 110 DEG C"]
["0725188","VALVE: TYPE: AIR VENT; VALVE SIZE: 3/4 X 3/8 IN; DESIGN RATING: 16 BAR; TEMPERATURE RATING: 120 DEG C; FACE TO FACE LENGTH: 1.5 MM; CONNECTION: INLET 3/4 NPT FEMALE X EXHAUSE 3/8 NPP FEMALE STRAIGHT; OPERATED: AIR; BODY MATERIAL: BRASS,INTERNAL: STAINLESS, SEAL :PEAK,NBR FKM; STYLE: POT SHAPED; TRIM: FLOAT TYPE AUTOMATIC; SOFTGOODS: O RING RUBBER; SPECIAL FEATURES: CALEFFI; MANUF P/N: 501500; ART 501","AUTOMATIC; Caleffi","AIR VENT","3/4 X 3/8 IN","BRASS,INTERNAL: STAINLESS, SEAL :PEAK,NBR FKM","16 BAR","FLOAT TYPE AUTOMATIC","INLET 3/4 NPT FEMALE X EXHAUSE 3/8 NPP FEMALE STRAIGHT","1.5 MM",null,"AIR",null,"120 DEG C"]
["0727285","VALVE: TYPE: FREE FLOATING LEVER AIR VENT; VALVE SIZE: 3/4 X 1/2 IN; DESIGN RATING: 21 BAR; TEMPERATURE RATING: 93 DEG C; FACE TO FACE LENGTH: 10.6 MM; CONNECTION: INLET 3/4 OUTLET 1/2 INCH; OPERATED: FLOAT; BODY MATERIAL: CAST IRON; STYLE: BOWL; SOFTGOODS: GRAPHITE GASKET (ITEM 9), 1.4301 WASHER (ITEM 14); MANUF P/N: 1AV ; SEAT, LEVERAGE SYSTEM, FLOAT STAINLESS STEEL, BODY AND CAP ASTM A48 CLASS 30 CAST IRON, GASKET GRAPHITE 60 X 75X 1 MM, BLOTS ASTM A193 GR B7, NUTS ASTM A563 GR A","ARMSTRONG INTERNATIONAL","FREE FLOATING LEVER AIR VENT","3/4 X 1/2 IN","CAST IRON","21 BAR",null,"INLET 3/4 OUTLET 1/2 INCH","10.6 MM",null,"FLOAT",null,"93 DEG C"]
["0738906","KIT, COMPRESSOR REPAIR: TYPE: SERVICE; APPLICATION: SPHERICAL VALVE; SPECIFICATION: ELECTRIC; COMPRISING: PISTON RINGS & GASKETS; MANUF P/N: 32226342; TYPE 30 MODEL 15T2, COMPRESSION STAGES 1, 2 AND 3, INGERSOLL RAND","TYPE 30; Ingersoll Rand","SERVICE",{"$nulls":8},"SPHERICAL VALVE"]
["0751644","VALVE, BALL: VALVE SIZE: 12 MM; DESIGN RATING: 400 BAR; TEMPERATURE RATING: -10 to +100 DEG C; CONNECTION: 1/2 IN; BODY MATERIAL: CARBON STEEL; FACE TO FACE LENGTH: 100 MM; OPERATED: LEVER; STYLE: SQUARE; TRIM: CARBON STEEL; SOFTGOODS: NONE; SPECIFICATION: 4 WAY BALL; PORT TYPE: STRAIGHT 1/2 INCH FITTING MALE TO FEMALE; APPLICATION: MAINTENANCE SEAL OPERATION","Parker Hannifin ","BALL; STRAIGHT 1/2 INCH FITTING MALE TO FEMALE","12 MM","CARBON STEEL","400 BAR","CARBON STEEL","1/2 IN","100 MM",null,"LEVER","MAINTENANCE SEAL OPERATION","-10 to +100 DEG C"]
["0751649","VALVE, BALL: VALVE SIZE: 12 MM; DESIGN RATING: 400 BAR; TEMPERATURE RATING: -10 to +100 DEG C; CONNECTION: 1/2'' STRAIGHT FEMALE FITTING; BODY MATERIAL: CS/CS-CS-POM; FACE TO FACE LENGTH: 100 MM; OPERATED: LEVER; STYLE: 3 WAY; TRIM: CARBON STEEL BALL ELEMENT; SOFTGOODS: NONE; SPECIFICATION: MULTI WAY BALL VALVE; PORT TYPE: 1/2 INCH FULL PORT IN; APPLICATION: OPERATING SEAL OPERATION; TYPE: ARGUS MW8","Argus","BALL; 1/2 INCH FULL PORT IN; ARGUS MW8","12 MM","CS/CS-CS-POM","400 BAR","CARBON STEEL BALL ELEMENT","1/2'' STRAIGHT FEMALE FITTING","100 MM",null,"LEVER","OPERATING SEAL OPERATION","-10 to +100 DEG C"]
["0783654","VALVE, GATE: VALVE SIZE: 80 MM; TYPE: GATE; DESIGN PRESSURE: 18 BAR; DESIGN TEMPERATURE: -120 TO 200 DEG C; CONNECTION: FLANGED DRILLED TO BS4504 PN 16; FACE TO FACE LENGTH: 223 MM; BODY MATERIAL: CAST IRON; TRIM: 8; OPERATED: HANDWHEEL; STEM DESIGN: RISING STEM; SPECIAL FEATURES: RESILIENT SEAT VALVE; AINSWORTH ,RAISED FACE,FIRE HYDRANT ,PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY","Ainsworth","GATE","80 MM","CAST IRON","18 BAR","8; RISING STEM","FLANGED DRILLED TO BS4504 PN 16","223 MM",null,"HANDWHEEL",null,"-120 TO 200 DEG C"]
["0783433","VALVE, GATE: VALVE SIZE: 150 MM; TYPE: SOLID WEGDE; DESIGN PRESSURE: 64 BAR; DESIGN TEMPERATURE: -20 to 200 DEG C; CONNECTION: FLANGED; FACE TO FACE LENGTH: 447 MM; BODY MATERIAL: CARBON STEEL; TRIM: 8; OPERATED: MANUAL HANDWHEEL; DIN 3352 T7,SPIRAL CASE DRAINAGE , PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY.","NEWAY","GATE; SOLID WEGDE","150 MM","CARBON STEEL","64 BAR","8","FLANGED","447 MM",null,"MANUAL HANDWHEEL",null,"-20 to 200 DEG C"]
["0783757","VALVE, DIAPHRAGM: TYPE: A; VALVE SIZE: 15 MM; DESIGN RATING: 16 BAR; TEMPERATURE RATING: -5 TO 100 DEG C; CONNECTION: SCREWED BSP THREADED FEMALE; BODY MATERIAL: CAST IRON; DIAPHRAGM MATERIAL: DIAPHRAGM GRADE Q; FACE TO FACE LENGTH: 64 MM; OPERATED: MANUAL; STYLE: TYPE A; SPECIFICATION: COATED; WATR TREATMENT, SAUNDERS WIER TYPE, SUPPLIER TO PROVIDE WITH THE PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATES.","Saunders","DIAPHRAGM; A","15 MM","CAST IRON; DIAPHRAGM GRADE Q","16 BAR","DIAPHRAGM GRADE Q","SCREWED BSP THREADED FEMALE","64 MM",null,"MANUAL",null,"-5 TO 100 DEG C"]
["0783432","VALVE, GATE: VALVE SIZE: 300 MM; TYPE: SOLID WEDGE WITH BYPASS; DESIGN PRESSURE: 63 BAR; DESIGN TEMPERATURE: -20 to 200 DEG C; CONNECTION: FLANGE FLAT FACE WITH O-RING GROOVE; FACE TO FACE LENGTH: 750 MM; BODY MATERIAL: CARBON STEEL; TRIM: 8; OPERATED: HANDWHEEL ACTUATED; STEM DESIGN: RISING STEM; APPLICATION: MANUAL BYPASS ISOLATING VALVE; SPECIAL FEATURES: WITH OPEN / CLOSE LEVEL INDICATOR; MANUF P/N: TYPE B3.35461; PRESSURE TESTING AND MATERIAL CERTIFICATE TO BE SUPPLIED UPON DELIVERY.","B3","GATE; SOLID WEDGE WITH BYPASS","300 MM","CARBON STEEL","63 BAR","8; RISING STEM","FLANGE FLAT FACE WITH O-RING GROOVE","750 MM",null,"HANDWHEEL ACTUATED","MANUAL BYPASS ISOLATING VALVE","-20 to 200 DEG C"]
["0783755","VALVE, BALL: VALVE SIZE: 12 MM; DESIGN RATING: 500 BAR; TEMPERATURE RATING: -45 TO 121 DEG C; CONNECTION: SCREWED TO BDP THREADED FEMALE; BODY MATERIAL: CARBON STEEL; FACE TO FACE LENGTH: 80 MM; OPERATED: MANUAL; TYPE: 2- WAY BALL VALVE; GOVE RECEIVER, PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATES.","Parker Hannifin ","BALL; 2- WAY BALL VALVE","12 MM","CARBON STEEL","500 BAR",null,"SCREWED TO BDP THREADED FEMALE","80 MM",null,"MANUAL",null,"-45 TO 121 DEG C"]
["0783664","VALVE: TYPE: 2-WAY; VALVE SIZE: 20 MM; DESIGN RATING: 420 BAR; TEMPERATURE RATING: -10 TO 80 DEG C; FACE TO FACE LENGTH: 95 MM; CONNECTION: SCREWED TO BSP THREADED FEMALE; OPERATED: MANUAL; BODY MATERIAL: CARBON STEEL; STYLE: BLOCK TYPE; GOV REC, THREADED FEMALE, SUPPLIER TO SUPPLY WITH THE PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATES.","Parker Hannifin/ HYDAC","2-WAY","20 MM","CARBON STEEL","420 BAR",null,"SCREWED TO BSP THREADED FEMALE","95 MM",null,"MANUAL",null,"-10 TO 80 DEG C"]
["0783762","VALVE, DIAPHRAGM: TYPE: A; VALVE SIZE: 25 MM; DESIGN RATING: 16 BAR; TEMPERATURE RATING: -5 TO 100 DEG C; CONNECTION: SCREWED TO BSP THREADED FEMALE; BODY MATERIAL: CAST IRON; DIAPHRAGM MATERIAL: GRADE 1; FACE TO FACE LENGTH: 108 MM; OPERATED: MANUAL; STYLE: TYPE A; SPECIFICATION: COATED; WATER TREATMENT, SAUNDERS WEIR TYPE, Q DIAPHRAGM, SUPPLIER TO SUPPLY WITH THE PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATES.","Saunders","DIAPHRAGM; A","25 MM","CAST IRON; GRADE 1","16 BAR","GRADE 1","SCREWED TO BSP THREADED FEMALE","108 MM",null,"MANUAL",null,"-5 TO 100 DEG C"]
["0750298","VALVE, RELIEF: VALVE SIZE: G3/4; SET PRESSURE: 48.5 BAR; TEMPERATURE RATING: -15 TO 200 DEG C; CONNECTION: G3/4 IN; BODY MATERIAL: BRASS; TRIM: BRASS; OPERATED: PRESSURE SPRING LOADED; MANUF P/N: PSB013-075; SAFETY VALVE TO BE SET AT 11 BAR (COLD SET PRESSURE). SAFETY VALVE TO BE TAGGED AND LED SEALED. INFORMATION ON TAG SHOULD CONTAIN:VALVE SERIAL NUMBER, SET PRESSURE, TEST DATE AND DUE DATE. DUE DATE SHOULD BE 3 YEARS FROM TEST DATE. VALVE. TEST REPORT TO BE SUPPLIED ALONG WITH VALVE.TEST REPORT TO DETAIL TO CORRESPOND WITH VALVE INFO","LESER","RELIEF","G3/4","BRASS","48.5 BAR","BRASS","G3/4 IN",null,null,"PRESSURE SPRING LOADED",null,"-15 TO 200 DEG C"]
["0783431","VALVE: TYPE: PLUG; VALVE SIZE: 300 MM; DESIGN RATING: 50 BAR; TEMPERATURE RATING: -20 to 200 DEG C; CONNECTION: FLANGED FLAT FACE WITH O-RING GROOVE; OPERATED: HYDRAULIC; BODY MATERIAL: CARBON STEEL; TRIM: 8; MANUF P/N: 2.53-18555; SPHERICAL VALVE BYPASS VALVE.PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY","NEWAY","PLUG","300 MM","CARBON STEEL","50 BAR","8","FLANGED FLAT FACE WITH O-RING GROOVE",null,null,"HYDRAULIC",null,"-20 to 200 DEG C"]
["0783759","VALVE, DIAPHRAGM: TYPE: A; VALVE SIZE: 50 MM; DESIGN RATING: 16 BAR; TEMPERATURE RATING: -5 TO 100 DEG C; CONNECTION: SCREWED T BSP THREADED FEMALE; BODY MATERIAL: CAST IRON; DIAPHRAGM MATERIAL: DIAPHRAGM GRADE Q; FACE TO FACE LENGTH: 165 MM; OPERATED: MANUAL; STYLE: TYPE A; SPECIFICATION: COATED; WATER TREATMENT, SAUNDERS WEIR TYPE, Q DIAPHRAGM, SUPPLIER TO SUPPLY WITH THE PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATES","Saunders","DIAPHRAGM; A","50 MM","CAST IRON; DIAPHRAGM GRADE Q","16 BAR","DIAPHRAGM GRADE Q","SCREWED T BSP THREADED FEMALE","165 MM",null,"MANUAL",null,"-5 TO 100 DEG C"]
["0765642","VALVE, GATE: VALVE SIZE: 100 MM; TYPE: SOLID WEDGE; DESIGN PRESSURE: 64 BAR; DESIGN TEMPERATURE: -20 to +400 DEG C; CONNECTION: FLANGED DIN 2513 FEMALE JOINT FLANGE ENDS; FACE TO FACE LENGTH: 350 MM; BODY MATERIAL: STAINLESS STEEL 304; TRIM: BODY SS304 ; BONNET SS304 ; WEDGE : SS304 ; SEAT : SS304 ; STEM : SS304; OPERATED: HANDWHEEL RISING SPINDLE; APPLICATION: PALMIET LABYRINTH SUPPLY ISOLATION; SPECIFICATION: DESIGN AS PER DIN3352 / EN1171; SPECIAL FEATURES: TO BE SUPPLIED WITH PRESSURE TEST AND MATERIAL CERTIFICATES; GRADE: STAINLESS STEEL 304","DATA NOT AVAILABLE","GATE; SOLID WEDGE","100 MM","STAINLESS STEEL 304","64 BAR","BODY SS304","FLANGED DIN 2513 FEMALE JOINT FLANGE ENDS","350 MM",null,"HANDWHEEL RISING SPINDLE","PALMIET LABYRINTH SUPPLY ISOLATION","-20 to +400 DEG C"]
["0780490","MANIFOLD: TYPE: 2 WAY VALVE MANIFOLD; MATERIAL: STAINLESS STEEL; MANUF P/N: P2/W4GW4GTV2AH-R; 2 VALVE BLOCK AND VENT GAUGE VALVE, PROCESS CONNECTION FEMALE 1/2” BSPG, INSTRUMENT CONNECTION FEMALE 1/2” BSPG, PTFE PACKING,1/4” NPT VENT PORT, ALL TAPS ANTI-TAMPER, 6000 PSI, 316 SS, M6 X 16MM PCD MOUNTING HOLES; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","No further information available","PROCESS CONNECTION FEMALE 1/2” BSPG, INSTRUMENT CONNECTION FEMALE 1/2” BSPG, PTFE PACKING,1/4” NPT VENT PORT, ALL TAPS ANTI-TAMPER, 6000 PSI, 316 SS, M6 X 16MM PCD MOUNTING HOLES; 2 WAY VALVE MANIFOLD",null,"STAINLESS STEEL",{"$nulls":4},"MOUNTING HOLES"]
["0783419","VALVE, GATE: VALVE SIZE: 50 MM; TYPE: GATE VALVE; DESIGN PRESSURE: 10 BAR; DESIGN TEMPERATURE: -29 TO 400 DEG C; CONNECTION: FLANGE DRILLED TO JIS 10K50; FACE TO FACE LENGTH: 140 MM; BODY MATERIAL: FCMB-535; TRIM: TRIM 8; OPERATED: MANUAL; HP INLET, GATE VALVE, SUPPLIER TO PROVE PRESSURE TEST CERTIFICATE AND THE MATERIAL PROPERTIES ON DELIVERY.","MALL","GATE; SUPPLIER TO PROVE PRESSURE TEST CERTIFICATE AND THE MATERIAL PROPERTIES ON DELIVERY; GATE VALVE","50 MM","FCMB-535","10 BAR","TRIM 8","FLANGE DRILLED TO JIS 10K50","140 MM",null,"MANUAL",null,"-29 TO 400 DEG C"]
["0783758","VALVE, DIAPHRAGM: TYPE: A; VALVE SIZE: 40 MM; DESIGN RATING: 16 BAR; TEMPERATURE RATING: -5 TO 100 DEG C; CONNECTION: FLANGE DRILLED TO BS4504 T16; BODY MATERIAL: CAST IRON; DIAPHRAGM MATERIAL: DIAPHRAGM GRADE Q; FACE TO FACE LENGTH: 165 MM; OPERATED: MANUAL; STYLE: TYPE A; SPECIFICATION: COATED; WATER TREATMENT, SAUNDERS WEIR TYPE, Q DIAPHRAGM, SUPPLIER TO SUPPLY WITH THE PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATES","Saunders","DIAPHRAGM; A","40 MM","CAST IRON; DIAPHRAGM GRADE Q","16 BAR","DIAPHRAGM GRADE Q","FLANGE DRILLED TO BS4504 T16","165 MM",null,"MANUAL",null,"-5 TO 100 DEG C"]
["0780491","MANIFOLD: TYPE: 3 VALVE DIRECT MOUNT MANIFOLD; MATERIAL: STAINLESS STEEL; MANUF P/N: S3/FTHAX-ZH; 3 WAY DIRECT MOUNT MANIFOLD, PTFE PACKING AND GASKET, 6000 PSI, 316 SS, ALL TAPS ANTI-TAMPER, O-RING TX HOOK-UP, 316 SS ASSEMBLY BOLT KIT INCLUDED; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","No further information available","3 VALVE DIRECT MOUNT MANIFOLD",null,"STAINLESS STEEL"]
["0783503","VALVE, GLOBE: VALVE SIZE: 80 MM; DESIGN PRESSURE: 2 - 21 BAR; DESIGN TEMPERATURE: 82 DEG C; FACE TO FACE LENGTH: 336 MM; OPERATED: SELF OPERATED; CONNECTION: FLANGE DRILLED TO BS4504 T16; BODY MATERIAL: STAINLESS STEEL; TRIM: STAINLESS STEEL; TYPE: PRESURE REDUCING GLOBE VALVE; MANUF P/N: 20868931A; OIL PURIFY BYPASS, PRESSURE REDUCING VALVE, FLANGE THICKNESS: 30MM, 8 BOLTS, CLA-VAL.CO, THIS VALVE INCLUDE 1 PRESSURE GAUGE, SST CRD PILOT AND TRIM & POSITION INDICATOR, SUPPLIER TO PROVIDE THE FOLLOWING ON DELIVERY: PRESURE TEST CERTIFICATE & MATERIAL PROPERTIES CERTIFICATE.","CLA-VAL.CO","GLOBE; FLANGE THICKNESS; PRESURE REDUCING GLOBE VALVE","80 MM","STAINLESS STEEL","2 - 21 BAR","STAINLESS STEEL","FLANGE DRILLED TO BS4504 T16","336 MM",null,"SELF OPERATED",null,"82 DEG C"]
["0683354","FLANGE: TYPE: DIESEL ENGINE AIR STARTING VALVE; DIMENSIONS: OD 152.4 MM; MATERIAL: CARBON STEEL; STYLE: RAISED FACE; GRADE: 304; SPECIFICATION: SABS 1123 1600/3; RAISED FACE = 3MM, OD = 152.4MM, ID = TO SUIT 50NB PIPE, PCD = 120.6MM, FLANGE THICKNESS = 25MM, NUMBER OF HOLES = 4, DIAMETER OF BOLT HOLES = 18MM","No further information available","DIESEL ENGINE AIR STARTING VALVE",null,"CARBON STEEL"]
["0783425","VALVE, CHECK: TYPE: CHECK VALVE; VALVE SIZE: 100 MM; DESIGN RATING: 40 BAR; TEMPERATURE RATING: -20 TO 120 DEG C; CONNECTION: FLANGE DRILLED TO BS4504 TABLE 40; BODY MATERIAL: WCB; FACE TO FACE LENGTH: 344 MM; OPERATED: SELF (SWING CHECK); BLOWDOWN AIR NON-RETURN VALVE, PERSTA, MODEL 240MT11.1, PRESSURE TESTING AND MATERIAL PROPERTIES TO SUPPLIED ON DELIVERY BY THE SUPPLIER.","PERSTA","CHECK; PERSTA, MODEL 240MT11.1, PRESSURE TESTING AND MATERIAL PROPERTIES TO SUPPLIED ON DELIVERY BY THE SUPPLIER; CHECK VALVE","100 MM","WCB","40 BAR",null,"FLANGE DRILLED TO BS4504 TABLE 40","344 MM",null,"SELF (SWING CHECK)",null,"-20 TO 120 DEG C"]
["0783437","VALVE: TYPE: GLOBE; VALVE SIZE: 100 MM; DESIGN RATING: 64 BAR; TEMPERATURE RATING: -20 TO 200 DEG C; FACE TO FACE LENGTH: 430 MM; CONNECTION: FLANGED & DRILLED TO EN1092-1; OPERATED: HYDRAULIC ACTUATOR WITH OPEN AND CLOSED POSITION SWITCH; BODY MATERIAL: CARBON STEEL; TRIM: 8; MANUF P/N: 2.41-48223; LABYRINTH COOLING WATER HYDRAULIC VALVE , PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY.","DATA NOT AVAILABLE","GLOBE","100 MM","CARBON STEEL","64 BAR","8","FLANGED & DRILLED TO EN1092-1","430 MM",null,"HYDRAULIC ACTUATOR WITH OPEN AND CLOSED POSITION SWITCH",null,"-20 TO 200 DEG C"]
["0783422","VALVE, GLOBE: VALVE SIZE: 50 MM; DESIGN PRESSURE: 40 BAR; DESIGN TEMPERATURE: -196 to 573 DEG C; FACE TO FACE LENGTH: 224 MM; OPERATED: MANUAL; CONNECTION: FLANGE DRILLED TO EN1092-1 TABLE 40; BODY MATERIAL: STAINLESS STEEL; TRIM: STAINLESS STEEL; INNER AND OUTER LAYBYRINTH, RAISED FACE WITH O-RING GROOVE, NON-RISING STEM, 200AF211, 1.0460, PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATE ON DELIVERY.","DATA NOT AVAILABLE","GLOBE","50 MM","STAINLESS STEEL","40 BAR","STAINLESS STEEL","FLANGE DRILLED TO EN1092-1 TABLE 40","224 MM",null,"MANUAL",null,"-196 to 573 DEG C"]
["0783760","VALVE, DIAPHRAGM: TYPE: A; VALVE SIZE: 80 MM; DESIGN RATING: 16 BAR; TEMPERATURE RATING: -5 to 100 DEG; CONNECTION: FLANGE DRILLED TO BS4504 T16; BODY MATERIAL: CAST IRON; DIAPHRAGM MATERIAL: DIAPHRAGM GRADE Q; FACE TO FACE LENGTH: 260 MM; OPERATED: MANUAL; STYLE: TYPE A; SPECIFICATION: COATED; WATER TREATMENT, SAUNDERS WEIR TYPE, Q DIAPHRAGM, SUPPLIER TO SUPPLY WITH THE PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATES","Saunders","DIAPHRAGM; A","80 MM","CAST IRON; DIAPHRAGM GRADE Q","16 BAR","DIAPHRAGM GRADE Q","FLANGE DRILLED TO BS4504 T16","260 MM",null,"MANUAL",null,"-5 to 100 DEG"]
["0783426","VALVE, BALL: VALVE SIZE: 80 MM; DESIGN RATING: 40 BAR; TEMPERATURE RATING: -40 TO 200 DEG C; CONNECTION: FLANGE DRILLED TO EN1092-1; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 180 MM; OPERATED: MANUAL; LEVEL INDICATOR L5 DRAFT TUBE, MODENTIC MD-27, DIN2635, RAISED FACE, PRESSURE TEST CERTIFICATE AND MATERIAL PROPERTIES CERTIFICATE TO BE SUPPLIED ON DELIVERY.","stewartsandlloydsvalves","BALL","80 MM","STAINLESS STEEL","40 BAR",null,"FLANGE DRILLED TO EN1092-1","180 MM",null,"MANUAL",null,"-40 TO 200 DEG C"]
["0783761","VALVE, DIAPHRAGM: TYPE: A; VALVE SIZE: 20 MM; DESIGN RATING: 16 BAR; TEMPERATURE RATING: -5 TO 100 DEG C; CONNECTION: SCREWED TO BSP THREADED FEMALE; BODY MATERIAL: CAST IRON; DIAPHRAGM MATERIAL: GRADE Q; FACE TO FACE LENGTH: 83 MM; OPERATED: MANUAL; STYLE: TYPE A; SPECIFICATION: COATED; WATER TREATMENT, SAUNDERS WEIR TYPE, Q DIAPHRAGM, SUPPLIER TO SUPPLY WITH THE PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATES","Saunders","DIAPHRAGM; A","20 MM","CAST IRON; GRADE Q","16 BAR","GRADE Q","SCREWED TO BSP THREADED FEMALE","83 MM",null,"MANUAL",null,"-5 TO 100 DEG C"]
["0783505","VALVE, BALL: VALVE SIZE: 50 MM; DESIGN RATING: 19 BAR; TEMPERATURE RATING: 5 - 75 DEG C; CONNECTION: FLANGED DRILLED TO BS4504 T16; BODY MATERIAL: WCB; FACE TO FACE LENGTH: 178 MM; OPERATED: MANUAL; TRIM: STAINLESS STEEL; TYPE: REDUCED BORE; OIL PURIFY, REDUCED BORE VALL VALE, CLASS 150, SERIES 500 BALL VALVE, IPVI, SUPPLIER TO PROVIDE WITH THE PRESSURE TEST CERTIFICATE AND A MATERIAL PROPERTIES CERTIFICATE.","IPV","BALL; IPVI, SUPPLIER TO PROVIDE WITH THE PRESSURE TEST CERTIFICATE AND A MATERIAL PROPERTIES CERTIFICATE; REDUCED BORE","50 MM","WCB","19 BAR","STAINLESS STEEL","FLANGED DRILLED TO BS4504 T16","178 MM",null,"MANUAL",null,"5 - 75 DEG C"]
["0783430","VALVE: TYPE: GLOBE; VALVE SIZE: 100 MM; DESIGN RATING: 40 BAR; TEMPERATURE RATING: -20 to 200 DEG C; FACE TO FACE LENGTH: 340 MM; CONNECTION: FLANGED DRILLED TO BS4504 TABLE 40; OPERATED: MANUAL HANDWHEEL; BODY MATERIAL: CARBON STEEL; TRIM: 8; BLOWDOWN AIR RECEIVER ISOLATION VALVE , PRESSURE TESTING AND MATERIAL CERTIDFICATES TO BE SUPPLIED UPON DELIVERY.","DATA NOT AVAILABLE","GLOBE","100 MM","CARBON STEEL","40 BAR","8","FLANGED DRILLED TO BS4504 TABLE 40","340 MM",null,"MANUAL HANDWHEEL",null,"-20 to 200 DEG C"]
["0783427","VALVE: TYPE: PLUG; VALVE SIZE: 40 MM; DESIGN RATING: 100 BAR; TEMPERATURE RATING: -20 to 200 DEG C; CONNECTION: FLANGED DRILLED TO EN1092-1; OPERATED: HYDRAULIC ACTUATOR WITH OPEN AND CLOSED POSITION SWITCH; BODY MATERIAL: CARBON STEEL; TRIM: 8; MANUF P/N: 2.41-48231; PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY.SHAFT SEAL HYDRAULIC VALVE","DATA NOT AVAILABLE","PLUG","40 MM","CARBON STEEL","100 BAR","8","FLANGED DRILLED TO EN1092-1",null,null,"HYDRAULIC ACTUATOR WITH OPEN AND CLOSED POSITION SWITCH",null,"-20 to 200 DEG C"]
["0768522","VALVE, GLOBE: VALVE SIZE: 15 MM; DESIGN PRESSURE: 10 KG/CM2; DESIGN TEMPERATURE: 180 DEG C; FACE TO FACE LENGTH: 85 MM; OPERATED: HANDWHEEL; CONNECTION: FLANGE; BODY MATERIAL: SCS13; TRIM: 18CR-8NI; SPECIFICATION: 10K-15 , KITZ , GLOBE VALVE","KITS","GLOBE","15 MM","SCS13","10 KG/CM2","18CR-8NI","FLANGE","85 MM",null,"HANDWHEEL",null,"180 DEG C"]
["0783792","VALVE, GATE: VALVE SIZE: 250 MM; TYPE: SOLID WEDGE; DESIGN PRESSURE: 16 BAR; DESIGN TEMPERATURE: 5 TO 40 DEG C; CONNECTION: FLANGED DRILLED TO BS4504 T16; FACE TO FACE LENGTH: 356 MM; BODY MATERIAL: CAST STEEL; TRIM: GUNMETAL; OPERATED: MANUAL HANDWHEEL; SPECIAL FEATURES: COPON LINED; DEWATERING, AINSWORTH RESILIENT SEAL GATE VALVE, NON-RISING SPINDLE WITH POSITION INDICATOR, PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATE TO BE SUPPLIED BY THE SUPPLIER ON DELIVERY.","Ainsworth","GATE; NON-RISING SPINDLE WITH POSITION INDICATOR, PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATE TO BE SUPPLIED BY THE SUPPLIER ON DELIVERY; SOLID WEDGE","250 MM","CAST STEEL","16 BAR","GUNMETAL","FLANGED DRILLED TO BS4504 T16","356 MM",null,"MANUAL HANDWHEEL",null,"5 TO 40 DEG C"]
["0783434","VALVE, GATE: VALVE SIZE: 300 MM; TYPE: SOLID WEDGE; DESIGN PRESSURE: 25 BAR; DESIGN TEMPERATURE: -20 to 200 DEG C; CONNECTION: FLANGED , DRILLED TO BS4504 PN25; FACE TO FACE LENGTH: 345 MM; BODY MATERIAL: CARBON STEEL; TRIM: 8; OPERATED: MANUAL HANDWHEEL; SPECIAL FEATURES: INTERNAL EPOXY COATED TO 400 UM; MANUF P/N: D300TS564CSEPO; UNIT CW , PRESSURE TESTING AND MATERIAL CERTIIFICATES TO BE SUPPLIED UPON DELIVERY.","DATA NOT AVAILABLE","GATE; SOLID WEDGE","300 MM","CARBON STEEL","25 BAR","8","FLANGED , DRILLED TO BS4504 PN25","345 MM",null,"MANUAL HANDWHEEL",null,"-20 to 200 DEG C"]
["0750300","VALVE, RELIEF: VALVE SIZE: DN 25; SET PRESSURE: 16.9 BAR; TEMPERATURE RATING: -15/200 DEG C; CONNECTION: 1\" BSP; BODY MATERIAL: BRASS; TRIM: BRASS; OPERATED: AUTOMATIC RELIEF AT SET PRESSURE; MANUF P/N: PSB013-074; SAFETY VALVE TO BE SET AT 16.94 BAR (COLD SET PRESSURE). SAFETY VALVE TO BE TAGGED AND LED SEALED. INFORMATION ON TAG SHOULD CONTAIN: VALVE SERIAL NUMBER, SET PRESSURE, TEST DATE AND DUE DATE. DUE DATE SHOULD BE 3 YEARS FROM TEST DATE. VALVE. TEST REPORT TO BE SUPPLIED ALONG WITH VALVE.TEST REPORT TO DETAIL TO CORRESPOND WITH VALVE INFO. TO SUIT 2ND STAGE ON COMPRESSOR MODEL V250-12-3N","TO SUIT 2ND STAGE ON COMPRESSOR","RELIEF","DN 25","BRASS","16.9 BAR","BRASS","1\" BSP",null,null,"AUTOMATIC RELIEF AT SET PRESSURE",null,"-15/200 DEG C"]
["0783756","VALVE, BALL: VALVE SIZE: 25 MM; DESIGN RATING: 420 BAR; TEMPERATURE RATING: -4 TO 121 DEG; CONNECTION: SCREWED TO BSP THREADED FEMALE; BODY MATERIAL: CARBON STEEL; FACE TO FACE LENGTH: 110 MM; OPERATED: MANUAL; GOV REC, THREADED FEMALE, PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATES TO BE SUPPLIED.","ARGUS","BALL","25 MM","CARBON STEEL","420 BAR",null,"SCREWED TO BSP THREADED FEMALE","110 MM",null,"MANUAL",null,"-4 TO 121 DEG"]
["0783435","VALVE: TYPE: PLUG; VALVE SIZE: 150 MM; DESIGN RATING: 64 BAR; TEMPERATURE RATING: -20 to 200 DEG C; CONNECTION: FLANGED & DRILLED TO EN1092-1; OPERATED: HYDRAULIC ACTUATOR WITH OPEN AND CLOSED POSITION SWITCH; BODY MATERIAL: CARBON STEEL; MANUF P/N: 2.41-48660; RUNNER BAND DRAIN HYDRAULIC VALVES , PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY","VOITH","PLUG","150 MM","CARBON STEEL","64 BAR",null,"FLANGED & DRILLED TO EN1092-1",null,null,"HYDRAULIC ACTUATOR WITH OPEN AND CLOSED POSITION SWITCH",null,"-20 to 200 DEG C"]
["0783423","VALVE, GATE: VALVE SIZE: 200 MM; TYPE: GATE VALVE; DESIGN PRESSURE: 10 BAR; DESIGN TEMPERATURE: -40 to 120 DEG C; CONNECTION: FLANGED; FACE TO FACE LENGTH: 290 MM; BODY MATERIAL: DUCTILE IRON; TRIM: STAINLESS STEEL; OPERATED: MANUAL; TGB ISOLATOR OIL, WORM & WHEEL GEAR STEM HANDLE WITH POSITION INDICATOR, RAISED FACE, BA-04P-P/N, SUMPLIER TO PROVIDE WITH THE PRESSURE TESTING & MATERIAL PROPERTIES CERTIFICATES.","DATA NOT AVAILABLE","GATE; GATE VALVE","200 MM","DUCTILE IRON","10 BAR","STAINLESS STEEL","FLANGED","290 MM",null,"MANUAL",null,"-40 to 120 DEG C"]
["0783754","VALVE, BALL: VALVE SIZE: 06 MM; DESIGN RATING: 500 BAR; TEMPERATURE RATING: -20 TO 60 DEG C; CONNECTION: THREADED FEMALE; BODY MATERIAL: STAINLESS STEEL; FACE TO FACE LENGTH: 70 MM; OPERATED: MANUAL; GOV COMPRESSOR BALL VALVE, PRESSURE TEST AND MATERIAL PROPERTIES","PERSTA","BALL; PRESSURE TEST AND MATERIAL PROPERTIES","06 MM","STAINLESS STEEL","500 BAR",null,"THREADED FEMALE","70 MM",null,"MANUAL",null,"-20 TO 60 DEG C"]
["0783421","VALVE, GATE: VALVE SIZE: 32 MM; TYPE: GATE VALVE; DESIGN PRESSURE: 10 BAR; DESIGN TEMPERATURE: -29 to 425 DEG C; CONNECTION: FLANGE DRILLED TO JIS 10K50; FACE TO FACE LENGTH: 120 MM; BODY MATERIAL: FCMB-535; TRIM: TRIM 8; OPERATED: MANUAL; HP OUTLET VALVE, PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATE ON DELIVERY.","MALL","GATE; PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATE ON DELIVERY; GATE VALVE","32 MM","FCMB-535","10 BAR","TRIM 8","FLANGE DRILLED TO JIS 10K50","120 MM",null,"MANUAL",null,"-29 to 425 DEG C"]
["0684520","VALVE: TYPE: SCREW DOWN NON-RETURN; VALVE SIZE: 1 IN; DESIGN RATING: 38 BAR; TEMPERATURE RATING: 100 DEG C; FACE TO FACE LENGTH: 241 MM; CONNECTION: FLANGED ENDS TO ANSI-300 LB; OPERATED: SWING, DISK; BODY MATERIAL: FORGED STEEL; STYLE: FLANGE BOLTED; TRIM: PLATNAM; SPECIFICATION: ANSI-300 LB (ASA); SOFTGOODS: GRAPHITE; SWING DISK","DATA NOT AVAILABLE","SCREW DOWN NON-RETURN","1 IN","FORGED STEEL","38 BAR","PLATNAM","FLANGED ENDS TO ANSI-300 LB","241 MM",null,"SWING, DISK",null,"100 DEG C"]
["0783436","VALVE: TYPE: GLOBE; VALVE SIZE: 65 MM; DESIGN RATING: 16 BAR; TEMPERATURE RATING: -20 to 200 DEG C; FACE TO FACE LENGTH: 288 MM; CONNECTION: FLANGED , DRILLED TO BS4504 TABLE 16; OPERATED: MANUAL HANDWHEEL; BODY MATERIAL: CARBON STEEL; TRIM: 8; PT GUIDE BEARING OIL ISOLATING VALVES , PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY.","DATA NOT AVAILABLE","GLOBE","65 MM","CARBON STEEL","16 BAR","8","FLANGED , DRILLED TO BS4504 TABLE 16","288 MM",null,"MANUAL HANDWHEEL",null,"-20 to 200 DEG C"]
["0783424","VALVE, GLOBE: VALVE SIZE: 25 MM; DESIGN PRESSURE: 40 BAR; DESIGN TEMPERATURE: -20 TO 120 DEG C; FACE TO FACE LENGTH: 155 MM; OPERATED: MANUAL; CONNECTION: FLANGE DRILLED TO BS4504 TYPE 40/2; BODY MATERIAL: STAINLESS STEEL; TRIM: STAINLESS STEEL; SHAFT SEAL VALVE, GLOBE VALVE, NON-RISING STEM, RAISED FACE, MODEL:200AE85.1, PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATE ON DELIVERY.","DATA NOT AVAILABLE","GLOBE; GLOBE VALVE, NON-RISING STEM, RAISED FACE, MODEL","25 MM","STAINLESS STEEL","40 BAR","STAINLESS STEEL","FLANGE DRILLED TO BS4504 TYPE 40/2","155 MM",null,"MANUAL",null,"-20 TO 120 DEG C"]
["0783504","VALVE, GLOBE: VALVE SIZE: 100 MM; DESIGN PRESSURE: 16 BAR; DESIGN TEMPERATURE: 400 DEG; FACE TO FACE LENGTH: 230 MM; OPERATED: MANUAL; CONNECTION: FLANGED DRILLED TO BS4504 T16; BODY MATERIAL: STAINLESS STEEL; TRIM: STAINLESS STEEL; MANUF P/N: GMK-GV-DN100-PN16-F2-WCB; TGB COOLER CW INLET & OUTLET VALVE, METAL VALVES(GMK), DIN3356, PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATES TO BE SUPPLIED ON DELIVERY.","GMK","GLOBE; METAL VALVES(GMK), DIN3356, PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATES TO BE SUPPLIED ON DELIVERY","100 MM","STAINLESS STEEL","16 BAR","STAINLESS STEEL","FLANGED DRILLED TO BS4504 T16","230 MM",null,"MANUAL",null,"400 DEG"]
["0783650","VALVE: TYPE: BELLOWS SEAL GLOBE; VALVE SIZE: 1/2 IN; DESIGN RATING: 30 KGF/CM2; TEMPERATURE RATING: -30 to 120 DEG C; FACE TO FACE LENGTH: 58 MM; CONNECTION: THREADED FEMALE ENDS; OPERATED: HANDWHEEL; BODY MATERIAL: BRASS; MANUF P/N: NBV1003; BRAKE AIR COMPRESSOR ,PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY","DATA NOT AVAILABLE","BELLOWS SEAL GLOBE","1/2 IN","BRASS","30 KGF/CM2",null,"THREADED FEMALE ENDS","58 MM",null,"HANDWHEEL",null,"-30 to 120 DEG C"]
["0774960","KIT: TYPE: PRESSURE RELIEF VALVES; APPLICATION: STANDBY DIESEL GENERAOTR; COMPRISING: PRESSURE RELIEF VALVE (15 BAR, 6-OFF);GROUP 015 TABLE 2/277-1;PART NUMBER:550 180 10 15,PRESSURE RELIEF VALVE (3-OFF);GROUP 016 TABLE 1/589-1;PART NUMBER:550 180 12 15.","DATA NOT AVAILABLE","PRESSURE RELIEF VALVES",{"$nulls":8},"STANDBY DIESEL GENERAOTR"]
["0783663","VALVE, CHECK: TYPE: NON RETURN; VALVE SIZE: 20 MM; DESIGN RATING: 16 BAR; TEMPERATURE RATING: -10 TO 120 DEG C; CONNECTION: SCREWED TO BSP TREADED FEMALE; BODY MATERIAL: BRONZE; FACE TO FACE LENGTH: 52 MM; OPERATED: SPRING; WATER TREATMENT PLANT, 2270 BRONZE, C/W RESILIENT SEAT, THREADED FEMALE, SUPPLIER TO SUPPLY WITH THE PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATES.","DATA NOT AVAILABLE","CHECK; NON RETURN","20 MM","BRONZE","16 BAR",null,"SCREWED TO BSP TREADED FEMALE","52 MM",null,"SPRING",null,"-10 TO 120 DEG C"]
["0783420","VALVE, GATE: VALVE SIZE: 250 MM; TYPE: GATE VALVE; DESIGN PRESSURE: 10 BAR; DESIGN TEMPERATURE: -29 TO 420 DEG C; CONNECTION: FLANGE DRILLED TO JIS 10K50; FACE TO FACE LENGTH: 332 MM; BODY MATERIAL: WCB; TRIM: TRIM 8; OPERATED: MANUAL; DUPLEX INLET AND OUTLET VALVE, DRILLED TO JIS10K250, RISING STEM, BA-OOP, WORN&WHEEL GEAR, STEM HANDWHEEL WITH POSITION INDICATOR, PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATE ON DELIVERY.","DATA NOT AVAILABLE","GATE; DRILLED TO JIS10K250, RISING STEM, BA-OOP, WORN&WHEEL GEAR, STEM HANDWHEEL WITH POSITION INDICATOR, PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATE ON DELIVERY; GATE VALVE","250 MM","WCB","10 BAR","TRIM 8","FLANGE DRILLED TO JIS 10K50","332 MM",null,"MANUAL",null,"-29 TO 420 DEG C"]
["0692548","VALVE, CHECK: TYPE: SWING DISK NRV; VALVE SIZE: 1 IN; DESIGN RATING: 300 LB; TEMPERATURE RATING: 38 DEG C; CONNECTION: FNPT; BODY MATERIAL: SS FORGED STEEL; FACE TO FACE LENGTH: 216 MM; OPERATED: AUTO; STYLE: THD BONNET; TRIM: BRASS; SOFTGOODS: SEAL NBR, BACK UP RING PTFE; APPLICATION: PREVENT BACKFLOW; SPECIFICATION: LB (ASA); GRADE: ANSI-300; FLANGED ENDS TO ANSI-300 LB (ASA)","DATA NOT AVAILABLE","CHECK; SWING DISK NRV","1 IN","SS FORGED STEEL","300 LB","BRASS","FNPT","216 MM",null,"AUTO","PREVENT BACKFLOW","38 DEG C"]
["0783648","VALVE, GLOBE: VALVE SIZE: 25 MM; DESIGN PRESSURE: 10 BAR; DESIGN TEMPERATURE: 120 DEG C; FACE TO FACE LENGTH: 127 MM; OPERATED: MANUAL; CONNECTION: FLANGED DRILLED TO JIS 10K; BODY MATERIAL: WCB; TRIM: 8; STEM DESIGN: NON RISING STEM; 10K25 ,UGB OIL COOLER ISOLATING VALVE, PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY","DATA NOT AVAILABLE","GLOBE; PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY","25 MM","WCB","10 BAR","8; NON RISING STEM","FLANGED DRILLED TO JIS 10K","127 MM",null,"MANUAL",null,"120 DEG C"]
["0783662","VALVE, CHECK: TYPE: WAFER; VALVE SIZE: 150 MM; DESIGN RATING: 16 BAR; TEMPERATURE RATING: 5 to 40 DEG C; CONNECTION: NO FLANGE; BODY MATERIAL: CAST IRON; FACE TO FACE LENGTH: 76 MM; OPERATED: AUTOMATIC; STYLE: WAFER; TRIM: COPON COATED; SOFTGOODS: EPDM; MANUF P/N: FIG 316; SEEPAGE PUMP DISCHARGE VALVE, WAFER TYPE, EPDM DIAPHRAGM, COPEN LINED, RIENZI, SUPPLIER TO SUPPLY WITH THE PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATES.","DATA NOT AVAILABLE","CHECK; WAFER TYPE, EPDM DIAPHRAGM, COPEN LINED, RIENZI, SUPPLIER TO SUPPLY WITH THE PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATES; WAFER","150 MM","CAST IRON","16 BAR","COPON COATED","NO FLANGE","76 MM",null,"AUTOMATIC",null,"5 to 40 DEG C"]
["0783651","VALVE, GLOBE: VALVE SIZE: 50 MM; DESIGN PRESSURE: 16 BAR; DESIGN TEMPERATURE: -120 to 200 DEG C; FACE TO FACE LENGTH: 225 MM; OPERATED: MANUAL; CONNECTION: FLANGED DRUILLED TO JIS 10K RAISED FACE; BODY MATERIAL: GG25; TRIM: 2; SPECIFICATION: NON RISING STEM; PT UPPER TANK , BODY AND SEAL PRESSURE TEST CERTIFICATES AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY","DATA NOT AVAILABLE","GLOBE","50 MM","GG25","16 BAR","2","FLANGED DRUILLED TO JIS 10K RAISED FACE","225 MM",null,"MANUAL",null,"-120 to 200 DEG C"]
["0783429","VALVE, CHECK: TYPE: SWING; VALVE SIZE: 50 MM; DESIGN RATING: 76 BAR; TEMPERATURE RATING: 538 DEG C; CONNECTION: FLANGED , DRILLED TO EN1092-1 PN 40; BODY MATERIAL: 316 SS; FACE TO FACE LENGTH: 265 MM; OPERATED: PRESSURE OPEN/CLOSE; SPECIFICATION: CLASS 300; NEWAY , BS1868,LABYRINTH COOLING WATER SYSTEM , PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY.","DATA NOT AVAILABLE","CHECK; SWING","50 MM","316 SS","76 BAR",null,"FLANGED , DRILLED TO EN1092-1 PN 40","265 MM",null,"PRESSURE OPEN/CLOSE",null,"538 DEG C"]
["0783504","VALVE, GLOBE: VALVE SIZE: 100 MM; DESIGN PRESSURE: 16 BAR; DESIGN TEMPERATURE: 400 DEG; FACE TO FACE LENGTH: 230 MM; OPERATED: MANUAL; CONNECTION: FLANGED DRILLED TO BS4504 T16; BODY MATERIAL: STAINLESS STEEL; TRIM: STAINLESS STEEL; MANUF P/N: GMK-GV-DN100-PN16-F2-WCB; TGB COOLER CW INLET & OUTLET VALVE, METAL VALVES(GMK), DIN3356, PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATES TO BE SUPPLIED ON DELIVERY.","GMK","GLOBE; METAL VALVES(GMK), DIN3356, PRESSURE TEST AND MATERIAL PROPERTIES CERTIFICATES TO BE SUPPLIED ON DELIVERY","100 MM","STAINLESS STEEL","16 BAR","STAINLESS STEEL","FLANGED DRILLED TO BS4504 T16","230 MM",null,"MANUAL",null,"400 DEG"]
["0783652","VALVE, GATE: VALVE SIZE: 250 MM; TYPE: SOLID WEDGE; DESIGN PRESSURE: 10 BAR; DESIGN TEMPERATURE: 120 DEG C; CONNECTION: FLANGED DRILLED TO JIS 10K; FACE TO FACE LENGTH: 329 MM; BODY MATERIAL: WCB; TRIM: 8; OPERATED: MANUAL - HANDWHEEL; STEM DESIGN: RISING STEM; APPLICATION: GEN COOLER CW ISOLATE; SPECIFICATION: 10K250; MANUF P/N: BA-00P; LIMITORQUE , HANDWHEEL ACTUATOR WORM AND GEAR SYSTEM.PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY","DATA NOT AVAILABLE","GATE; SOLID WEDGE","250 MM","WCB","10 BAR","8; RISING STEM","FLANGED DRILLED TO JIS 10K","329 MM",null,"MANUAL - HANDWHEEL","GEN COOLER CW ISOLATE","120 DEG C"]
["0783647","VALVE, GATE: VALVE SIZE: 80 MM; TYPE: SOLID WEDGE; DESIGN PRESSURE: 10 BAR; DESIGN TEMPERATURE: 120 DEG C; CONNECTION: FLANGED DRILLED TO JIS 10K; FACE TO FACE LENGTH: 200 MM; BODY MATERIAL: WCB; TRIM: 8; OPERATED: HANDWHEEL MANUAL OPERATED; STEM DESIGN: RISING STEM; UPPER GUIDE BEARING OIL ISOLATE,PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY","DATA NOT AVAILABLE","GATE; SOLID WEDGE","80 MM","WCB","10 BAR","8; RISING STEM","FLANGED DRILLED TO JIS 10K","200 MM",null,"HANDWHEEL MANUAL OPERATED",null,"120 DEG C"]
["0784003","VALVE, RELIEF: VALVE SIZE: 1 IN; SET PRESSURE: 600 KPA G; TEMPERATURE RATING: -20 TO -260 DEG C; CONNECTION: THREADED 1G MALE INLET 1G FEMALE OUTLET; BODY MATERIAL: BRASS; TRIM: STAINLESS/BRONZE; FACE TO FACE LENGTH: 44 MM; OPERATED: PRESSURE SPRING RELEASE; APPLICATION: FIRE PUMP RELIEF VALVES; STYLE: RIGHT ANGLED SAFETY VALVE; TYPE 485 BAILEY BIRKETT, PRESSURE SET TO 600KPA , PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY.","DATA NOT AVAILABLE","RELIEF","1 IN","BRASS","600 KPA G","STAINLESS/BRONZE","THREADED 1G MALE INLET 1G FEMALE OUTLET","44 MM",null,"PRESSURE SPRING RELEASE","FIRE PUMP RELIEF VALVES","-20 TO -260 DEG C"]
["0784000","VALVE, BUTTERFLY: TYPE: WAFER; VALVE SIZE: 6 IN; DESIGN RATING: 20.7 BAR; TEMPERATURE RATING: 100 DEG C; CONNECTION: CLAMPED; BODY MATERIAL: DUCTILE IRON; FACE TO FACE LENGTH: 61 MM; OPERATED: HANDWHEEL AND GEAR ACTUATED; TRIM: NYLON-RILSON FIRE POWDERS (PA11)BLACK; SOFTGOODS: EPDM ENCAPSULATED; APPLICATION: FIRE WATER SYSTEM TEST VALVE; SPECIAL FEATURES: UL & FM APPROVED CE CERTIFIED; MANUF P/N: BFV 300; TYCO","Tyco Fire Products (Johnson Controls)","BUTTERFLY; WAFER","6 IN","DUCTILE IRON","20.7 BAR","NYLON-RILSON FIRE POWDERS (PA11)BLACK","CLAMPED","61 MM",null,"HANDWHEEL AND GEAR ACTUATED","FIRE WATER SYSTEM TEST VALVE","100 DEG C"]
["0784005","VALVE, GATE: VALVE SIZE: 200 MM; TYPE: SOLID WEDGE; DESIGN PRESSURE: 16 BAR; DESIGN TEMPERATURE: 5 TO 40 DEG C; CONNECTION: FLANGED DRILLED TO BS4504 T16; FACE TO FACE LENGTH: 317 MM; BODY MATERIAL: SPHEROIDAL GRAPHITE IRON; TRIM: 8; OPERATED: MANUAL HANDWHEEL; APPLICATION: FIRE RESERVOIR INLET; SPECIAL FEATURES: RESILIENT SEAT VALVE; PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY","DATA NOT AVAILABLE","GATE; SOLID WEDGE","200 MM","SPHEROIDAL GRAPHITE IRON","16 BAR","8","FLANGED DRILLED TO BS4504 T16","317 MM",null,"MANUAL HANDWHEEL","FIRE RESERVOIR INLET","5 TO 40 DEG C"]
["0784002","VALVE, GATE: VALVE SIZE: 250 MM; TYPE: SOLID WEDGE; DESIGN PRESSURE: 16 BAR; DESIGN TEMPERATURE: 5 TO 40 DEG C; CONNECTION: FLANGED DRILLED TO BS4504 T16; FACE TO FACE LENGTH: 380 MM; BODY MATERIAL: SPHEROIDAL GRAPHITE IRON; TRIM: 8; OPERATED: MANUAL HANDWHEEL; APPLICATION: FIRE PUMP INLET AND OUTLET; SPECIAL FEATURES: RESILIENT SEAT VALVE; PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY,AINSWORTH","Ainsworth","GATE; SOLID WEDGE","250 MM","SPHEROIDAL GRAPHITE IRON","16 BAR","8","FLANGED DRILLED TO BS4504 T16","380 MM",null,"MANUAL HANDWHEEL","FIRE PUMP INLET AND OUTLET","5 TO 40 DEG C"]
["0784001","VALVE, GATE: VALVE SIZE: 2 IN; TYPE: SOLID WEDGE; DESIGN PRESSURE: 20 BAR; DESIGN TEMPERATURE: -20 to 200 DEG C; CONNECTION: THREADED FEMALE BOTH ENDS BSPP; FACE TO FACE LENGTH: 74 MM; BODY MATERIAL: BRASS ALLOY; TRIM: BRASS; OPERATED: HAND WHEEL OPERATED; APPLICATION: JOCKEY FIRE PUMP ISOLATING VALVE; PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY","DLM","GATE; SOLID WEDGE","2 IN","BRASS ALLOY","20 BAR","BRASS","THREADED FEMALE BOTH ENDS BSPP","74 MM",null,"HAND WHEEL OPERATED","JOCKEY FIRE PUMP ISOLATING VALVE","-20 to 200 DEG C"]
["0784004","VALVE, CHECK: TYPE: SPRING; VALVE SIZE: 50 MM; DESIGN RATING: 18 BAR; TEMPERATURE RATING: -20 to 200 DEG C; CONNECTION: THREADED BSPP FEMALE BOTH ENDS; BODY MATERIAL: BRASS ALLOY; FACE TO FACE LENGTH: 101 MM; OPERATED: PRESSURE OPERATED; APPLICATION: JOCKEY FIRE PUMP NRV; MANUF P/N: ITAP 21-2; EUROPA , PRESSURE TESTING AND MATERIAL CERTIFICATES TO BE SUPPLIED UPON DELIVERY","Europa / ITAP","CHECK; SPRING","50 MM","BRASS ALLOY","18 BAR",null,"THREADED BSPP FEMALE BOTH ENDS","101 MM",null,"PRESSURE OPERATED","JOCKEY FIRE PUMP NRV","-20 to 200 DEG C"]

{"sheet":"Port Rex Gas Turbine","index":14,"n_rows":9,"n_cols":14,"rows_kept":9}
["Material","Original Description","OEM / Manufacturer","Valve Type","Size","Body Material","Class / Rating","Trim / Internals","End Connection","Face-to-Face","Drilling / PCD","Operation","Medium / Service","Medium Temperature"]
["0023886","VALVE, BUTTERFLY: TYPE: WAFER; VALVE SIZE: 150 MM; CONNECTION: FLANGE; BODY MATERIAL: STL; OPERATED: AIR; TRIM: DISC STL; ACTUATOR/ASSY,BLEED","Wood Group Pratt & Whitney Industrial Turbine Services, LLC (WGPW)","BUTTERFLY; WAFER","150 MM","STL",null,"DISC STL","FLANGE",null,null,"AIR"]
["0023887","VALVE, BUTTERFLY: TYPE: WAFER; VALVE SIZE: 150 MM; CONNECTION: FLANGE; BODY MATERIAL: STL; OPERATED: AIR; TRIM: DISC STL; ACTUATOR AND VALVE ASSY; BLEED","Wood Group Pratt & Whitney Industrial Turbine Services, LLC (WGPW)","BUTTERFLY; WAFER","150 MM","STL",null,"DISC STL","FLANGE",null,null,"AIR"]
["0023899","VALVE: TYPE: CONTROL; ASSY; AIR STARTER","Wood Group Pratt & Whitney Industrial Turbine Services, LLC (WGPW)","CONTROL"]
["0023905","VALVE, SOLENOID: PIPE SIZE: 25 MM; STYLE: 2 WAY; POTENTIAL: 110 VAC; 120 VDC; DESIGN RATING: 115/225/300 KPA; CONNECTION: FNPT; BODY MATERIAL: BRASS; OPERATED: AIR; ENCLOSURE RATING: IP67; MEDIUM: AIR/GAS/WATER; POWER: 20 W; ORIFICE SIZE: 25 MM; FREQUENCY 50/60 HZ, FOR USE ON COMPRESSOR",null,"SOLENOID","25 MM","BRASS","115/225/300 KPA",null,"FNPT",null,null,"AIR","AIR/GAS/WATER; COMPRESSOR"]
["0062790","VALVE, SOLENOID: PIPE SIZE: 8 MM; STYLE: 2 WAY; POTENTIAL: 120 VAC; DESIGN RATING: 150 LB; CONNECTION: FNPT; BODY MATERIAL: STEEL; MEDIUM: AIR/LIQUID; POWER: 10 W; ORIFICE SIZE: 1/16 X 3/64 IN; 60 HZ; GENERAL PURPOSE ENCLOSURE",null,"SOLENOID","8 MM; 1/16 X 3/64 IN","STEEL","150 LB",null,"FNPT",{"$nulls":3},"AIR/LIQUID"]
["0074427","SEAL, RING: TYPE: VALVE END; INSIDE DIAMETER: 58 MM; OUTSIDE DIAMETER: 62 MM; THICKNESS: 3 MM; MATERIAL: TEFLON; APPLICATION: VALVE; REFERENCE NO: 20117-16",null,"VALVE END",null,"TEFLON",{"$nulls":6},"VALVE"]
["0256828","VALVE: TYPE: LIQUID FUEL METERING; VALVE SIZE: 193.5 MM2; DESIGN RATING: 345 KPA; TEMPERATURE RATING: -28 TO +103 DEG C; CONNECTION: BASE; OPERATED: ELECTRICAL; BODY MATERIAL: METAL; MANUF P/N: LQ25, 9907-361; SUPPL P/N: LQ25T","Wood Group Pratt & Whitney Industrial Turbine Services, LLC (WGPW)","LIQUID FUEL METERING","193.5 MM2","METAL","345 KPA",null,"BASE",null,null,"ELECTRICAL",null,"-28 TO +103 DEG C"]
["0589427","VALVE, RELIEF: VALVE SIZE: 3/4 IN; SET PRESSURE: 420 KPA; TEMPERATURE RATING: 70 DEG C; CONNECTION: THD 1/2 IN; BODY MATERIAL: BRASS; TRIM: PLASTIC BONNET/ADJUSTABLE SCREW; FACE TO FACE LENGTH: 65 MM; OPERATED: PRESSURE 0-460 KPA; DESIGN RATING: 40 BAR; PRESSURE RANGE: 0-40 BAR; MANUF P/N: D22-1/2A",null,"RELIEF","3/4 IN","BRASS","40 BAR; 0-40 BAR; 420 KPA","PLASTIC BONNET/ADJUSTABLE SCREW","THD 1/2 IN","65 MM",null,"PRESSURE 0-460 KPA",null,"70 DEG C"]

{"sheet":"Sere Wind Farm","index":15,"n_rows":2,"n_cols":14,"rows_kept":2}
["Material","Original Description","OEM / Manufacturer","Valve Type","Size","Body Material","Class / Rating","Trim / Internals","End Connection","Face-to-Face","Drilling / PCD","Operation","Medium / Service","Medium Temperature"]
["0621484","VALVE, BUTTERFLY: TYPE: LUG WAFER; VALVE SIZE: 150 MM; DESIGN RATING: PN16; TEMPERATURE RATING: 0-120 DEG C; CONNECTION: LUG; BODY MATERIAL: DI; FACE TO FACE LENGTH: 59 MM; OPERATED: ACTUATOR; TRIM: RUBBER LINED; SOFTGOODS: SEAL; APPLICATION: TURBINE PROTECTION; GRADE: GGG40; SHAFT CONNECTION: DIA 14MM","Kennedy Valves","BUTTERFLY; LUG WAFER","150 MM","DI","PN16","RUBBER LINED","LUG; DIA 14MM","59 MM",null,"ACTUATOR","TURBINE PROTECTION","0-120 DEG C"]

{"sheet":"Vanderkloof Hydro Power","index":16,"n_rows":3,"n_cols":14,"rows_kept":3}
["Material","Original Description","OEM / Manufacturer","Valve Type","Size","Body Material","Class / Rating","Trim / Internals","End Connection","Face-to-Face","Drilling / PCD","Operation","Medium / Service","Medium Temperature"]
["0062654","VALVE, GATE: VALVE SIZE: 200 MM; TYPE: SOLID WEDGE; CONNECTION: FLANGE; BODY MATERIAL: CI; TRIM: BONNET CI; OPERATED: HANDWHEEL; STEM DESIGN: RISING OUTSIDE SCREW; STYLE: BOLTED BONNET; SUPPL P/N: Y1501-11","HITACHI","GATE; SOLID WEDGE","200 MM","CI",null,"BONNET CI; RISING OUTSIDE SCREW","FLANGE",null,null,"HANDWHEEL"]
["0062793","VALVE, SOLENOID: PIPE SIZE: 100 MM; STYLE: 2 WAY; POTENTIAL: 110/120 VAC; DESIGN RATING: 2.5 MPA; CONNECTION: FLANGE; BODY MATERIAL: STEEL; OPERATED: SOLENOID; ENCLOSURE RATING: IP 65 (EN 60529); MEDIUM: WATER; POWER: 220 VAC; CURRENT: 0.45 A; APPLICATION: GEN BEARING COOLER CW FLOW CONTROL; SPECIFICATION: PED; MANUF P/N: 8651000.9504.22050; REFERENCE NO: 27148735 & 27148736; SOLENOID VALVE INCLUDING A PISTON TYPE 2-WAY VALVE AND ELECTRICAL SOLENOID; DUTY CYCLE: 100% ED; VOLTAGE: FREQUENCY: 50HZ; VALVE MECHANICAL DETAILS: VALVE TYPE: 2/2 WAY PISTON VALVE; OPERATING PRESSURE: 0 - 25 BAR; RATED FLOW RATE: 125 M3/H = 34.7 L/S;VALVE MECHANICAL INTERFACE (FLANGE) DETAILS: FLANGE-TO-FLANGE FACE DIMENSION: 350MM; FLANGE STANDARD AND CLASS/TABLE: 100NB BS 4504 16/3;FLANGE OD = Ø220.0MM; RAISED FACE DIAMETER = Ø158.0MM; RAISED FACE HEIGHT = 3.0MM; NUMBER OF BOLTS = 8; BOLT HOLE DIAMETER = Ø18.0MM.","NORGREN","SOLENOID; 2/2 WAY PISTON VALVE","100 MM","STEEL","2.5 MPA",null,"FLANGE","350MM","BOLT HOLE DIAMETER = Ø18; 100NB BS 4504 16/3","SOLENOID","WATER; GEN BEARING COOLER CW FLOW CONTROL"]