Sentech Content and Media Operations IP Managed Switched Outlet PDU

# Project Overview:

Sentech Content and Media Operations require IP Managed Switched Outlets PDU to power the new EFC Racks.

# Specifications:

The following are the specifications for the PDUs that will be installed:

• Power Distribution Units (PDUs): 4 x units of IP Managed Switched Outlet PDUs, with minimum of 20 Switched Power Outlets(IEC) per PDU.

**Note: Each PDU should be Managed by Web Browser or Application and terminate on 32A 2P plus earth Industrial Plug**.

# Scope of Work:

The scope of work for this project includes several key activities:

1. Installation of PDUs supplied.
2. On- Site Demonstration of how the PDUs IP Address is configured
3. On- Site Demonstration of how the PDUs power outlets are switched individually remotely(Web Browser or Application)
4. Provide full documentation of the PDUs, Datasheets and Manuals
5. Perform User Acceptance Tests that will demonstrate all the Mandatory Criteria Items 1 to 6.

**Administrative Compliance Before Site Handover:**

1. Completion of OHS/Safety file spec & sect 37 agreement to be provided
2. National Key Point Security Clearance of the person(s) for on-site for installations