{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Data"],"read":"whole","date_system":"1900"}

{"sheet":"Data","index":0,"n_rows":234,"n_cols":5,"rows_kept":234}
["Material","Text","Base Unit of Measure","Quantity ","Price "]
[4501,"FUSE, CARTRIDGE: CURRENT: 16 A; POTENTIAL: 415 VAC; CONNECTION TYPE: BLADE KNIFE; DIMENSIONS: DIA 14 X LG 60 MM; TYPE: TIME LAG MEDIUM; CASE MATERIAL: CERAMIC; SUPPL P/N: NS16; FUSE, CARTRIDGE; CURRENT 16 A, POTENTIAL 415 VAC, DIMENSIONS DIA 14 X LG 60 MM, TYPE TIME LAG MEDIUM, CASE MATERIAL CERAMIC, CONNECTION TYPE BLADE KNIFE, PART NUMBER: NS16~FUSE,CARTD;NS16,16 A,415 VAC,CERAMIC","EA",275]
[4504,"FUSE, CARTRIDGE: CURRENT: 2 A; POTENTIAL: 415 V; CONNECTION TYPE: BLADE KNIFE; DIMENSIONS: DIA 14 X LG 60 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: GLASS; SPECIFICATION: BS 88 IEC 60269; SUPPL P/N: NS2; FUSE, CARTRIDGE; CURRENT 2 A, POTENTIAL 415 V, DIMENSIONS DIA 14 X LG 60 MM, TYPE CURRENT LIMITING, CASE MATERIAL GLASS, CONNECTION TYPE BLADE KNIFE, PART NUMBER: NS2 FUSE,CARTD; NS2,2 A,415 V,BLADE KNIFE; BS 88 OR IEC 60 269 CERTIFIED; FUSE BODY LENGTH 56.4 MM; BREAKING RANGE AND UTILIZATION CATEGORY: GG; SIZE: A3","EA",611]
[4507,"FUSE, CARTRIDGE: CURRENT: 6 A; POTENTIAL: 415 VAC; CONNECTION TYPE: BLADE KNIFE; DIMENSIONS: DIA 14 X LG 60 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; SUPPL P/N: NS6A; SUPPLIER NOTE, THE ITEM MUST BE ORIGINAL PROTECTIVE PACKED","EA",925]
[4509,"FUSE, CARTRIDGE: CURRENT: 10 A; POTENTIAL: 415 V; CONNECTION TYPE: BLADE KNIFE; DIMENSIONS: DIA 14 X LG 60 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; SPECIFICATION: BS 88 IEC 60269; SUPPL P/N: NS10A; FUSE, CARTRIDGE; CURRENT 10 A, POTENTIAL 415 V, DIMENSIONS DIA 14 X LG 60 MM, TYPE CURRENT LIMITING, CASE MATERIAL CERAMIC, CONNECTION TYPE BLADE KNIFE, PART NUMBER: NS10A FUSE,CARTD;NS10A,10 A,415 V,BLADE KNIFE; BS 88 OR IEC 60 269 CERTIFIED; FUSE BODY LENGTH 56.4 MM; BREAKING RANGE AND UTILIZATION CATEGORY: GG; SIZE: A3","EA",1200]
[4527,"FUSE, CARTRIDGE: CURRENT: 20 A; POTENTIAL: 240 V; CONNECTION TYPE: BLADE KNIFE TAGS; DIMENSIONS: DIA 12 X LG 47 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; SUPPL P/N: SS20; FUSE, CARTRIDGE; CURRENT 20 A, POTENTIAL 240 V, DIMENSIONS DIA 12 X LG 47 MM, TYPE CURRENT LIMITING, CASE MATERIAL CERAMIC, CONNECTION TYPE BLADE KNIFE TAGS, PART NUMBER: SS20~FUSE,CARTD;SS20,20 A,240 V,CERAMIC","EA",10]
[4530,"FUSE, CARTRIDGE: CURRENT: 25 A; POTENTIAL: 415 V; CONNECTION TYPE: BLADE KNIFE; DIMENSIONS: DIA 14 X LG 35 MM; TYPE: FAST BLOW; CASE MATERIAL: GLASS; SPECIFICATION: BS 88-1967; SUPPL P/N: NS25; HRC, CLASS Q1, ASTA CERTIFIED FOR CATEGORY OF DUTY 415AC80","EA",480]
[4537,"FUSE, CARTRIDGE: CURRENT: 200 A; POTENTIAL: 500 VAC; CONNECTION TYPE: BLADE KNIFE; DIMENSIONS: WD 46.6 X LG 132.6 MM; TYPE: INDICATING; CASE MATERIAL: CERAMIC; SPECIFICATION: NH1; REFERENCE NO: 3NA3140","EA",526]
[4538,"FUSE, CARTRIDGE: CURRENT: 160 A; POTENTIAL: 500 VAC; CONNECTION TYPE: BLADE KNIFE; DIMENSIONS: WD 28 X LG 78 X HT 42 MM; TYPE: INDICATING; CASE MATERIAL: CERAMIC; SUPPL P/N: 3NA3836; FUSE, CARTRIDGE; CURRENT 160 A, POTENTIAL 500 VAC, DIMENSIONS WD 28 X LG 78 X HT 42 MM, TYPE INDICATING, CASE MATERIAL CERAMIC, CONNECTION TYPE BLADE KNIFE, PART NUMBER: 3NA3836~FUSE,CARTD;3NA3836,160 A,500 VAC","EA",149]
[4540,"FUSE, CARTRIDGE: CURRENT: 40 A; POTENTIAL: 500 VAC; CONNECTION TYPE: BLADE KNIFE; DIMENSIONS: WD 21 X LG 79 X HT 40 MM; TYPE: INDICATING; CASE MATERIAL: CERAMIC; MANUF P/N: 3NA3817","EA",274]
[4544,"FUSE, CARTRIDGE: CURRENT: 80 A; POTENTIAL: 500 VAC; CONNECTION TYPE: BLADE KNIFE; DIMENSIONS: WD 40 X LG 46 MM; TYPE: INDICATING; CASE MATERIAL: CERAMIC; SUPPL P/N: 3NA3824","EA",389]
[4658,"FUSE, CARTRIDGE: CURRENT: 4 A; POTENTIAL: 415 VAC; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 13.9 X LG 55.6 MM; TYPE: INDICATING; CASE MATERIAL: CERAMIC; REFERENCE NO: NIT4; HIGH RUPTURING, CAPACITY","EA",294]
[117135,"FUSE, CARTRIDGE: CURRENT: 2 A; POTENTIAL: 500 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 23 X LG 50 MM; TYPE: FAST BLOW INDICATING; CASE MATERIAL: CERAMIC; REFERENCE NO: 1000504/2A; DIAZED, QUICK RESPONSE, COMP PUMP","EA",181]
[117136,"FUSE, CARTRIDGE: CURRENT: 1.6 A; POTENTIAL: 250 VAC; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 4 X LG 20 MM; TYPE: INDICATING; CASE MATERIAL: GLASS; SUPPL P/N: CEB-1.6A","EA",10]
[117137,"FUSE, CARTRIDGE: CURRENT: 100 MA; POTENTIAL: 250 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 6.3 X LG 32 MM; TYPE: MINIATURE, FAST BLOW; CASE MATERIAL: GLASS","EA",10]
[117138,"FUSE, CARTRIDGE: CURRENT: 250 MA; POTENTIAL: 250 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 6.3 X LG 32 MM; TYPE: MINIATURE, FAST BLOW; CASE MATERIAL: GLASS","EA",15]
[117139,"FUSE, CARTRIDGE: CURRENT: 500 MA; POTENTIAL: 250 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 6.3 X LG 32 MM; TYPE: MINIATURE; CASE MATERIAL: GLASS; SUPPL P/N: 3AG; CURRENT LIMITING","EA",20]
[117140,"FUSE, CARTRIDGE: CURRENT: 1 A; POTENTIAL: 250 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 6.3 X LG 32 MM; TYPE: FAST BLOW; CASE MATERIAL: GLASS; SUPPL P/N: 6332 LT; CURRENT LIMITING","EA",20]
[117141,"FUSE, CARTRIDGE: CURRENT: 2.5 A; POTENTIAL: 250 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 6 X LG 32 MM; TYPE: MINIATURE, FAST BLOW; CASE MATERIAL: GLASS","EA",20]
[117142,"FUSE, CARTRIDGE: CURRENT: 4 A; POTENTIAL: 250 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 6.3 X LG 32 MM; TYPE: MINIATURE, FAST BLOW; CASE MATERIAL: GLASS; SUPPL P/N: 6332 LT","EA",34]
[117143,"FUSE, CARTRIDGE: CURRENT: 2 A; POTENTIAL: 250 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 6 X LG 32 MM; TYPE: FAST BLOW; CASE MATERIAL: GLASS","EA",10]
[117144,"FUSE, CARTRIDGE: CURRENT: 2 A; POTENTIAL: 250 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 5 X LG 20 MM; TYPE: SLO BLOW; CASE MATERIAL: GLASS; REFERENCE NO: 19195","EA",48]
[117145,"FUSE, CARTRIDGE: CURRENT: 2 A; POTENTIAL: 220 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 5 X LG 20 MM; TYPE: FAST BLOW; CASE MATERIAL: GLASS; SUPER FLINK","EA",450]
[117146,"FUSE, CARTRIDGE: CURRENT: 10 A; POTENTIAL: 250 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 5 X LG 20 MM; TYPE: SLO BLOW; CASE MATERIAL: GLASS","EA",1]
[117147,"FUSE, CARTRIDGE: CURRENT: 15 A; POTENTIAL: 250 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 6.3 X LG 32 MM; TYPE: SLO BLOW; CASE MATERIAL: GLASS","EA",10]
[117148,"FUSE, CARTRIDGE: CURRENT: 50 A; POTENTIAL: 250 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 5 X LG 20 MM; TYPE: SLO BLO, MINIATURE; CASE MATERIAL: GLASS","EA",15]
[117149,"FUSE, CARTRIDGE: CURRENT: 5 A; POTENTIAL: 250 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 5 X LG 20 MM; TYPE: FAST BLOW; CASE MATERIAL: GLASS","EA",12]
[117150,"FUSE, CARTRIDGE: CURRENT: 6.3 A; POTENTIAL: 500 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 5 X LG 20 MM; TYPE: FAST BLOW; CASE MATERIAL: GLASS","EA",10]
[117151,"FUSE, CARTRIDGE: CURRENT: 10 A; POTENTIAL: 250 V; DIMENSIONS: DIA 5 X LG 20 MM; TYPE: FAST BLOW; CASE MATERIAL: PORCELAIN; AMHERD TYPE, SUPER FLINK","EA",15]
[117152,"FUSE, CARTRIDGE: CURRENT: 20 A; POTENTIAL: 600 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 21 X LG 127 MM; TYPE: TIME DELAY DUAL ELEMENT; CASE MATERIAL: FIBER; REFERENCE NO: TRS25R","EA",20]
[117153,"FUSE, CARTRIDGE: CURRENT: 25 A; POTENTIAL: 600 VAC; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 21 X LG 127 MM; TYPE: TIME DELAY DUAL ELEMENT; CASE MATERIAL: FIBER; REFERENCE NO: TS25R","EA",25]
[117154,"FUSE, CARTRIDGE: CURRENT: 15 A; POTENTIAL: 600 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 20.5 X LG 126 MM; TYPE: TIME DELAY INDICATING; CASE MATERIAL: CERAMIC; REFERENCE NO: TRS15R; RELIANCE R5K","EA",120]
[117155,"FUSE, CARTRIDGE: CURRENT: 315 A; POTENTIAL: 550 VAC; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 50 X LG 135 MM; TYPE: ONE TIME REJECTION; CASE MATERIAL: CERAMIC; LOW VOLTAGE, HRC, GEC, CLASS Q1, CATEGORY OF DUTY 550AC80, BS DIAMETER REFERENCE B3, 111 MM FIX CENTRES, TO BS88 1975, TO THE LATEST EDITION OF SABS 172 AND BEARING THE SABS MARK OF APPROVAL","EA",195]
[117156,"FUSE, CARTRIDGE: CURRENT: 3 A; POTENTIAL: 250 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 6.3 X LG 25 MM; TYPE: MINIATURE, FAST BLOW; CASE MATERIAL: CERAMIC; CURRENT LIMITING; GLASS TUBE, SIZE 5MM DIAMETER X 20MM LONG","EA",10]
[117218,"FUSE, CARTRIDGE: CURRENT: 4 A; POTENTIAL: 415 VAC; CONNECTION TYPE: BLADE KNIFE; DIMENSIONS: DIA 14 X LG 60 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; SUPPL P/N: NS4; SUPPLIER NOTE, THE ITEM MUST BE PROTECTIVE PACKED AND CLEARLY MARKED","EA",430]
[117220,"FUSE, CARTRIDGE: CURRENT: 6 A; POTENTIAL: 550 VAC; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 14 X LG 54 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; SUPPL P/N: NIT6; ONE SIDE, TWO HOLES","EA",180]
[117221,"FUSE, CARTRIDGE: CURRENT: 6 A; POTENTIAL: 660 VAC; CONNECTION TYPE: SCREW CLAMP OFFSET HOLE; DIMENSIONS: DIA 22 X LG 84 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; SUPPL P/N: TIA6; 73 MM HOLE CENTRES","EA",795]
[117224,"FUSE, CARTRIDGE: CURRENT: 10 A; POTENTIAL: 550 V; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 22 X LG 86 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; SPECIFICATION: BS 88; SUPPL P/N: TIA10; FUSE BODY LENGTH 56.4 MM; BREAKING RANGE AND UTILIZATION CATEGORY: GG; SIZE: A2","EA",25]
[117225,"FUSE, CARTRIDGE: CURRENT: 16 A; POTENTIAL: 415 VAC; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 22 X LG 84 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; SPECIFICATION: BS 88 IEC 60269; SUPPL P/N: TIA16; SUPPLIER NOTE, THE ITEM MUST BE PROTECTIVE PACKED AND CLEARLY MARKED; BS 88 OR IEC 60 269 CERTIFIED; FUSE BODY LENGTH 56.4 MM; BREAKING RANGE AND UTILIZATION CATEGORY: GG; SIZE: A3","EA",250]
[117226,"FUSE, CARTRIDGE: CURRENT: 20 A; POTENTIAL: 415 VAC; CONNECTION TYPE: BLADE KNIFE; DIMENSIONS: DIA 13.9 X LG 60.3 MM; INTERRUPT CAPACITY: 80 KA; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; SPECIFICATION: BS 88 IEC 60269; SUPPL P/N: NS20; FUSE, CARTRIDGE; CURRENT 20 A, POTENTIAL 415 VAC, DIMENSIONS DIA 13.9 X LG 60.3 MM, TYPE CURRENT LIMITING, CASE MATERIAL CERAMIC, CONNECTION TYPE BLADE KNIFE, PART NUMBER: NS20~FUSE, CARTD; NS20,20 A,415 VAC, CERAMIC; BS 88 OR IEC 60 269 CERTIFIED; FUSE BODY LENGTH 56.4 MM; BREAKING RANGE AND UTILIZATION CATEGORY: GG; SIZE: A3","EA",180]
[117227,"FUSE, CARTRIDGE: CURRENT: 20 A; POTENTIAL: 415 VAC; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 22 X LG 84 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; SPECIFICATION: BS 88 IEC 60269; SUPPL P/N: TIA20; SUPPLIER NOTE, THE ITEM MUST BE PROTECTIVE PACKED AND CLEARLY MARKED; BS 88 OR IEC 60 269 CERTIFIED; FUSE BODY LENGTH 56.4 MM; BREAKING RANGE AND UTILIZATION CATEGORY: GG; SIZE: A3","EA",555]
[117229,"FUSE, CARTRIDGE: CURRENT: 25 A; POTENTIAL: 550 VAC; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 22 X LG 80 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; SUPPL P/N: TIA25; SUPPLIER NOTE, THE ITEM MUST BE PROTECTIVE PACKED AND CLEARLY MARKED; BS 88 OR IEC 60 269 CERTIFIED; FUSE BODY LENGTH 56.4 MM; BREAKING RANGE AND UTILIZATION CATEGORY: GG; SIZE: A3","EA",17]
[117232,"FUSE, CARTRIDGE: CURRENT: 63 A; POTENTIAL: 550 V; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 22 X LG 85 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; SPECIFICATION: BS 88-1967; SUPPL P/N: TIS63; CLASS Q1","EA",490]
[117233,"FUSE, CARTRIDGE: CURRENT: 80 A; POTENTIAL: 550 VAC; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 26.2 X LG 111 MM; INTERRUPT CAPACITY: 80 KA; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; SPECIFICATION: BS 88 IEC 60269; SUPPL P/N: TCP80; OFF-SET TAGS 2-HOLE FIXING; FUSE BODY LENGTH: 58 MM; BREAKING RANGE AND UTILIZATION CATEGORY: GG; SIZE: A4","EA",340]
[117234,"FUSE, CARTRIDGE: CURRENT: 100 A; POTENTIAL: 550 VAC; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 26 X LG 110 MM; INTERRUPT CAPACITY: 80 KA; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; SPECIFICATION: BS 2692; IEC 282-1; SUPPL P/N: TCP100","EA",200]
[117236,"FUSE, CARTRIDGE: CURRENT: 200 A; POTENTIAL: 550 VAC; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 40 X LG 135 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; SUPPL P/N: TF200","EA",105]
[117239,"FUSE, CARTRIDGE: CURRENT: 400 A; POTENTIAL: 550 VAC; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 56 X LG 210 MM; INTERRUPT CAPACITY: 80 KA; TYPE: INDICATING; CASE MATERIAL: CERAMIC; SPECIFICATION: BS 88 IEC 60269; SUPPL P/N: TM400; BS 88 OR IEC 60 269 CERTIFIED; FUSE BODY LENGTH 56.4 MM; BREAKING RANGE AND UTILIZATION CATEGORY: GG; SIZE: A3","EA",60]
[117240,"FUSE, CARTRIDGE: CURRENT: 500 A; POTENTIAL: 550 VAC; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 85 X LG 212 MM; INTERRUPT CAPACITY: 80 KA; TYPE: INSTANTANEOUS; CASE MATERIAL: CERAMIC; SPECIFICATION: BS 88 IEC 60269; SUPPL P/N: TTM/FFM500; NORMAL INSTANTANEOUS OPERATING; BS 88 OR IEC 60 269 CERTIFIED; FUSE BODY HEIGHT 85 MM; BREAKING RANGE AND UTILIZATION CATEGORY: GG; SIZE: C2","EA",27]
[117243,"FUSE, CARTRIDGE: CURRENT: 100 A; POTENTIAL: 22 KV; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 61 X LG 355 MM; TYPE: INDICATING; CASE MATERIAL: CERAMIC; REFERENCE NO: LEL OHGMA11/12; 6/87 3XD; HRC, HIGH VOLTAGE OPEN FUSE CUT OUT","EA",34]
[117268,"FUSE, CARTRIDGE: CURRENT: 36 A; POTENTIAL: 550 VAC; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 22 X LG 85 MM; INTERRUPT CAPACITY: 80 KA; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; SPECIFICATION: BS 88 IEC 60269; SUPPL P/N: TIS36; BS 88 OR IEC 60 269 CERTIFIED; FUSE BODY LENGTH 56.4 MM; BREAKING RANGE AND UTILIZATION CATEGORY: GG; SIZE: A3","EA",3]
[117269,"FUSE, CARTRIDGE: CURRENT: 100 MA; POTENTIAL: 250 VAC; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 5 X LG 20 MM; TYPE: FAST BLOW; CASE MATERIAL: GLASS","EA",15]
[117271,"FUSE, CARTRIDGE: CURRENT: 125 A; POTENTIAL: 250 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 5 X LG 20 MM; TYPE: MINIATURE, FAST BLOW; CASE MATERIAL: GLASS; SUPPL P/N: FSF034-1507; REFERENCE NO: F125MA250V","EA",10]
[117274,"FUSE, CARTRIDGE: CURRENT: 500 MA; POTENTIAL: 250 VAC; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 5 X LG 20 MM; TYPE: FAST BLOW; CASE MATERIAL: GLASS; SPECIFICATION: DIN 41661; REFERENCE NO: DIN41661; FSF034-1513","EA",550]
[117278,"FUSE, CARTRIDGE: CURRENT: 800 MA; POTENTIAL: 250 VAC; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 5 X LG 20 MM; TYPE: FAST BLOW; CASE MATERIAL: GLASS","EA",700]
[117299,"FUSE, CARTRIDGE: CURRENT: 10 A; POTENTIAL: 125-250 VAC; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 6.3 X LG 32 MM; TYPE: FAST BLOW; CASE MATERIAL: GLASS; SUPPL P/N: 632-027; WITH EXTINGUISHING AGENT","EA",25]
[117304,"FUSE, CARTRIDGE: CURRENT: 75 A; POTENTIAL: 240 V; CONNECTION TYPE: SCREW CLAMP OFFSET TAGS; DIMENSIONS: DIA 17.4 X LG 34 MM; TYPE: FAST BLOW; CASE MATERIAL: CERAMIC; REFERENCE NO: GSA75; GS","EA",17]
[117306,"FUSE, CARTRIDGE: CURRENT: 125 A; POTENTIAL: 550 VAC; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 40 X LG 110 MM; TYPE: INDICATING; CASE MATERIAL: CERAMIC; SUPPL P/N: TFP125; REFERENCE NO: 5000401; HRC","EA",397]
[117307,"FUSE, CARTRIDGE: CURRENT: 125 A; POTENTIAL: 550 VAC; 460 VDC; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 40 X LG 135 MM; INTERRUPT CAPACITY: 80 KA; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; SPECIFICATION: BS 88 IEC 60269; SUPPL P/N: TO BS 66-2; TF125; REFERENCE NO: B2; CLASS Q; BS 88 OR IEC 60 269 CERTIFIED; FUSE BODY LENGTH 56.4 MM; BREAKING RANGE AND UTILIZATION CATEGORY: GG; SIZE: A3","EA",272]
[117309,"FUSE, CARTRIDGE: CURRENT: 160 A; POTENTIAL: 660 VAC; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 34 X LG 134 MM; INTERRUPT CAPACITY: 80 KA; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; SPECIFICATION: BS 88 IEC 60269; SUPPL P/N: TF160; BS 88 OR IEC 60 269 CERTIFIED; FUSE BODY LENGTH 56.4 MM; BREAKING RANGE AND UTILIZATION CATEGORY: GG; SIZE: A3","EA",204]
[117310,"FUSE, CARTRIDGE: CURRENT: 315 A; POTENTIAL: 550 VAC; CONNECTION TYPE: SCREW CLAMP CENTER TAGS; DIMENSIONS: DIA 41 X LG 159 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; SUPPL P/N: TKM315; REFERENCE NO: 50 011 01; DUTY 80, CLASS Q1, WITH FIXING HOLES","EA",109]
[117321,"FUSE, CARTRIDGE: CURRENT: 80 A; POTENTIAL: 415 V; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 35 X LG 109 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; SPECIFICATION: BS 88-5; HRC, Q1","EA",15]
[117322,"FUSE, CARTRIDGE: CURRENT: 100 A; POTENTIAL: 415 V; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 40 X LG 114 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; SPECIFICATION: BS 88; HRC LINK, LIST NUMBER: AC80, CLASS Q1, SIBA BRAND ONLY","EA",17]
[117325,"FUSE, CARTRIDGE: CURRENT: 250 A; POTENTIAL: 550 VAC; 460 VDC; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 50 X LG 135 MM; INTERRUPT CAPACITY: 80 KA; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; SPECIFICATION: BS 88 IEC 60269; SUPPL P/N: TKF250; BS 88 OR IEC 60 269 CERTIFIED; FUSE BODY LENGTH 56.4 MM; BREAKING RANGE AND UTILIZATION CATEGORY: GG; SIZE: A3","EA",161]
[117327,"FUSE, CARTRIDGE: CURRENT: 500 A; POTENTIAL: 415 VAC; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 55 X LG 130 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; SUPPL P/N: JSU500; REFERENCE NO: JS500","EA",6]
[117330,"FUSE, CARTRIDGE: CURRENT: 25 A; POTENTIAL: 11 KVAC; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 51 X LG 460 MM; TYPE: INDICATING; CASE MATERIAL: CERAMIC; REFERENCE NO: ADGHC","EA",25]
[117336,"FUSE, CARTRIDGE: CURRENT: 16 A; POTENTIAL: 11-12 KV; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 63.5 X LG 255 MM; TYPE: INDICATING; CASE MATERIAL: CERAMIC; SPECIFICATION: BS 2692-1956 AMENDMENT 5; SINGLE","EA",10]
[117337,"FUSE, CARTRIDGE: CURRENT: 36 A; POTENTIAL: 7.2-12 KV; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 64 X LG 254 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; REFERENCE NO: KEBX036; TYPE GEC, HRC, FREE AIR RATING 32 AMP","EA",7]
[117338,"FUSE, CARTRIDGE: CURRENT: 50 A; POTENTIAL: 12 KV; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 64 X LG 250 MM; TYPE: INDICATING; CASE MATERIAL: CERAMIC; LINK, STRIKER","EA",8]
[117344,"FUSE, CARTRIDGE: CURRENT: 125 A; POTENTIAL: 250 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 5 X LG 20 MM; TYPE: SLO BLOW; CASE MATERIAL: GLASS; SUPPL P/N: FST034-3108","EA",150]
[117348,"FUSE, CARTRIDGE: CURRENT: 500 MA; POTENTIAL: 250 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 6 X LG 25 MM; TYPE: FAST BLOW; CASE MATERIAL: GLASS; REFERENCE NO: F312","EA",27]
[117359,"FUSE, CARTRIDGE: CURRENT: 16 A; POTENTIAL: 415 V; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 14 X LG 55 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; SUPPL P/N: NIT16; SUPPLIER NOTE, THE ITEM MUST BE PROTECTIVE PACKED AND CLEARLY MARKED","EA",330]
[117361,"FUSE, CARTRIDGE: CURRENT: 20 A; POTENTIAL: 415 VAC; 250 VDC; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 14 X LG 55 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; SUPPL P/N: NIT20; TAG ONE SIDE, TWO HOLES","EA",130]
[117379,"FUSE, CARTRIDGE: CURRENT: 250 A; POTENTIAL: 550 VAC; CONNECTION TYPE: CENTER TAGS; DIMENSIONS: ID 50 X LG 150 MM; INTERRUPT CAPACITY: 80 KA; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; SUPPL P/N: TKM250; HRC, LIST NO 50 011 01, CODE Q1, 2 HOLE FIXING","EA",62]
[117385,"FUSE, CARTRIDGE: CURRENT: 200 MA; POTENTIAL: 250 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 5 X LG 20 MM; TYPE: FAST BLOW; CASE MATERIAL: GLASS; REFERENCE NO: FSF034-1509","EA",30]
[117519,"FUSE, CARTRIDGE: CURRENT: 100 A; POTENTIAL: 550 VAC; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 33 X LG 108 MM; INTERRUPT CAPACITY: 80 KA; TYPE: TIME DELAY; CASE MATERIAL: CERAMIC; SPECIFICATION: BS 88 PART 1; SHORT TIME AMP 160, MOTOR BRUSH","EA",137]
[117525,"FUSE, CARTRIDGE: CURRENT: 25 A; POTENTIAL: 660 VAC; CONNECTION TYPE: BLADE KNIFE; DIMENSIONS: WD 48 X LG 50 X HT 30 MM; TYPE: INDICATING; CASE MATERIAL: PORCELAIN; SUPPL P/N: 3NE8015; REFERENCE NO: 2020920/25","EA",47]
[117526,"FUSE, CARTRIDGE: CURRENT: 6 A; POTENTIAL: 500 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 22 X LG 51 MM; TYPE: BOTTLE INDICATING; CASE MATERIAL: CERAMIC; SUPPL P/N: 5SA231; DIAZED, HOBART 136203-3","EA",10]
[117527,"FUSE, CARTRIDGE: CURRENT: 3.15 A; POTENTIAL: 250 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 5 X LG 20 MM; TYPE: FAST BLOW; CASE MATERIAL: GLASS","EA",10]
[117528,"FUSE, CARTRIDGE: CURRENT: 100 A; POTENTIAL: 550 V; CONNECTION TYPE: BLADE KNIFE; DIMENSIONS: WD 21 X LG 79 X HT 35 MM; TYPE: INDICATING; CASE MATERIAL: CERAMIC; SPECIFICATION: DIN 43620; VDE 0636/21; REFERENCE NO: 2000013/100A","EA",158]
[117529,"FUSE, CARTRIDGE: CURRENT: 35 A; POTENTIAL: 550 V; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 22 X LG 85 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; SPECIFICATION: BS 88; SUPPL P/N: TIS35AX; REFERENCE NO: TIS35","EA",522]
[117530,"FUSE, CARTRIDGE: CURRENT: 2 A; POTENTIAL: 500 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 22 X LG 50 MM; TYPE: BOTTLE INDICATING; CASE MATERIAL: CERAMIC; REFERENCE NO: 136203-2ISH; 10005004","EA",15]
[117533,"FUSE, CARTRIDGE: CURRENT: 200 A; POTENTIAL: 550 V; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 40 X LG 109.4 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; SPECIFICATION: BS 88-1975; REFERENCE NO: TCP250; HRC, LIST NUMBER: 5000401, CLASS Q1","EA",5]
[117534,"FUSE, CARTRIDGE: CURRENT: 200 A; POTENTIAL: 660 V; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 33.4 X LG 135.7 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; SPECIFICATION: BS 88-2; SUPPL P/N: 317632; CLASS Q1, B2","EA",20]
[117535,"FUSE, CARTRIDGE: CURRENT: 160 A; POTENTIAL: 415-550 VAC; 460 VDC; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 40 X LG 108 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; SPECIFICATION: BS 88-1975; REFERENCE NO: TF160AX; B2; LOW VOLTAGE HRC, CATEGORY OF DUTY 550AC80, BS DIA, FIX CENTRES 111MM","EA",10]
[117536,"FUSE, CARTRIDGE: CURRENT: 315 A; POTENTIAL: 550 VAC; 460 VDC; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 48 X LG 155 MM; TYPE: ONE TIME REJECTION; CASE MATERIAL: CERAMIC; SPECIFICATION: BS 88-1975; REFERENCE NO: 5001101/1; LOW VOLTAGE, SIBA, CLASS Q1, CATEGORY OF DUTY 550AC80 MAXIMUM, FIX CENTRES 133MM","EA",113]
[117537,"FUSE, CARTRIDGE: CURRENT: 100 A; POTENTIAL: 415-550 VAC; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 36 X 135 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; SPECIFICATION: SABS 172; LOW VOLTAGE HRC, CLASS Q1, TO THE LATEST EDITION OF SABS 172 AND BEARING THE SABS MARK OF APPROVAL","EA",13]
[117538,"FUSE, CARTRIDGE: CURRENT: 125 A; POTENTIAL: 415 V; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 40 X LG 134 MM; TYPE: INDICATING; CASE MATERIAL: CERAMIC; SPECIFICATION: BS 88-2-1975; REFERENCE NO: B2; HRC, LIST NUMBER 5000901, CLASS Q1","EA",16]
[117539,"FUSE, CARTRIDGE: CURRENT: 80 A; POTENTIAL: 550 VAC; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 31 X LG 135 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; SPECIFICATION: BS 88-1975; IEC 269-2; SABS 172; SUPPL P/N: TC; LOW VOLTAGE HRC, CLASS Q1, TO THE LATEST EDITION OF SABS 172 AND BEARING THE SABS MARK OF APPROVAL","EA",423]
[117543,"FUSE, CARTRIDGE: CURRENT: 10 A; POTENTIAL: 300 VAC; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 10.2 X LG 33.4 MM; TYPE: TIME DELAY; CASE MATERIAL: CERAMIC; REFERENCE NO: SC10; LOW VOLTAGE, CLASS G","EA",15]
[117548,"FUSE, CARTRIDGE: CURRENT: 25 A; POTENTIAL: 660 VAC; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 14 X LG 51 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; REFERENCE NO: GOULD-17539","EA",20]
[117549,"FUSE, CARTRIDGE: CURRENT: 6.3 A; POTENTIAL: 500 VAC; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 5 X LG 30 MM; TYPE: MEDIUM TIME LAG; CASE MATERIAL: GLASS; REFERENCE NO: 19405; CURRENT LIMITING; BREAKING CAPACITY C","EA",10]
[117550,"FUSE, CARTRIDGE: CURRENT: 800 MA; POTENTIAL: 500 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 5 X LG 30 MM; TYPE: MEDIUM TIME DELAY; CASE MATERIAL: GLASS; CURRENT LIMITING","EA",10]
[117551,"FUSE, CARTRIDGE: CURRENT: 2 A; POTENTIAL: 500 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 5 X LG 30 MM; TYPE: MEDIUM TIME LAG; CASE MATERIAL: GLASS","EA",10]
[117552,"FUSE, CARTRIDGE: CURRENT: 160 A; POTENTIAL: 660 V; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: WD 30 X LG 79 X HT 45 MM; TYPE: INDICATING; CASE MATERIAL: CERAMIC; SUPPL P/N: 3/83/48 VK; VERSION 1 00-80","EA",10]
[117553,"FUSE, CARTRIDGE: CURRENT: 63 A; POTENTIAL: 660 V; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: WD 27 X LG 103 X HT 44 MM; INTERRUPT CAPACITY: 100 KA; TYPE: INDICATING; CASE MATERIAL: CERAMIC; SPECIFICATION: ISO 9001; REFERENCE NO: VDE0636-23; WITH TWO STEEL LIFE LUGS","EA",10]
[117554,"FUSE, CARTRIDGE: CURRENT: 400 A; POTENTIAL: 250 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 5 X LG 20 MM; TYPE: MINIATURE TIME DELAY MEDIUM; CASE MATERIAL: GLASS; SUPPL P/N: CFP; CURRENT LIMITING","EA",10]
[117568,"FUSE, CARTRIDGE: CURRENT: 4 A; POTENTIAL: 500 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 22 X LG 50 MM; TYPE: TIME LAG INDICATING; CASE MATERIAL: CERAMIC; REFERENCE NO: 5SB221; DIAZED, E27 THREAD","EA",20]
[117570,"FUSE, CARTRIDGE: CURRENT: 2 A; POTENTIAL: 250 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 5 X LG 20 MM; TYPE: MINIATURE ANTI SURGE; CASE MATERIAL: GLASS","EA",10]
[117571,"FUSE, CARTRIDGE: CURRENT: 2 A; POTENTIAL: 250 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 5 X LG 25 MM; TYPE: MINIATURE, FAST BLOW; CASE MATERIAL: GLASS","EA",10]
[117574,"FUSE, CARTRIDGE: CURRENT: 25 A; POTENTIAL: 550 VAC; CONNECTION TYPE: SCREW CLAMP OFFSET TAGS; DIMENSIONS: DIA 12 X LG 85 MM; INTERRUPT CAPACITY: 80 KA; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; SPECIFICATION: ISO 9001; REFERENCE NO: TIA 50-00101","EA",509]
[117575,"FUSE, CARTRIDGE: CURRENT: 4 A; POTENTIAL: 550 V; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 22 X LG 84 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; SPECIFICATION: BS 88-1975; SABS 172; REFERENCE NO: A2; TIA4; LOW VOLTAGE, HRC, BS DIAMETER, FIX CENTRES 73MM CATEGORY OF DUTY 550AC80, TO THE LATEST EDITION OF SABS 172 AND BEARING THE SABS MARK OF APPROVAL","EA",504]
[117576,"FUSE, CARTRIDGE: CURRENT: 2 A; POTENTIAL: 550 VAC; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 22 X LG 84 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; REFERENCE NO: TIA2AX","EA",561]
[117585,"FUSE, CARTRIDGE: CURRENT: 32 A; POTENTIAL: 380 VAC; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 10 X LG 38 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: PORCELAIN; REFERENCE NO: IFO 4006232","EA",149]
[117586,"FUSE, CARTRIDGE: CURRENT: 2 A; POTENTIAL: 220 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 5 X LG 20 MM; TYPE: FAST BLOW; CASE MATERIAL: GLASS","EA",160]
[117592,"FUSE, CARTRIDGE: CURRENT: 100 A; POTENTIAL: 600 V; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 25.5 X LG 112 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: FIBER; REFERENCE NO: A60X100","EA",10]
[117593,"FUSE, CARTRIDGE: CURRENT: 50 A; POTENTIAL: 600 V; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 21 X LG 110 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: FIBER; REFERENCE NO: A60X50","EA",40]
[117599,"FUSE, CARTRIDGE: CURRENT: 3 A; POTENTIAL: 7.2-12 KV; DIMENSIONS: DIA 25.5 X LG 194 MM; CASE MATERIAL: CERAMIC; CULLINAN ELECTRICAL, TYPE OMDNN, B8558, END CAPS 31MM LONG BOTH ENDS","EA",20]
[117600,"FUSE, CARTRIDGE: CURRENT: 3 A; POTENTIAL: 3.3 KV; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 22.2 X LG 143.2 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; ENGLISH ELECTRIC, LIST NUMBER AIR 3.3/3A","EA",20]
[117609,"FUSE, CARTRIDGE: CURRENT: 355 A; POTENTIAL: 3-7.2 KV; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 76.8 X LG 360 MM; TYPE: INDICATING; CASE MATERIAL: CERAMIC; SPECIFICATION: DIN 282/21; DIN 43625; WITH STRIKER PIN, E=292 MM","EA",15]
[117610,"FUSE, CARTRIDGE: CURRENT: 50 A; POTENTIAL: 2 KV; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 52 X LG 258 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; REFERENCE NO: S208850A; S2088; HRC","EA",11]
[117612,"FUSE, CARTRIDGE: CURRENT: 125 A; POTENTIAL: 500 VAC; CONNECTION TYPE: BLADE KNIFE; DIMENSIONS: WD 29 X LG 148 X HT 42 MM; TYPE: INDICATING; CASE MATERIAL: CERAMIC; SPECIFICATION: VDE0636; REFERENCE NO: 3NA4232","EA",195]
[117613,"FUSE, CARTRIDGE: CURRENT: 630 A; POTENTIAL: 550 V; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 74 X LG 211 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; TYPE C2TTM630X, 3NE 1434 FS 6, SPARES FOR STATION BATTERY CHARGER B1-B6 550","EA",10]
[117614,"FUSE, CARTRIDGE: CURRENT: 315 A; POTENTIAL: 800 VAC; CONNECTION TYPE: KNIFE BLADE W/SLOTS; DIMENSIONS: SQ 60 X LG 142 MM; TYPE: INDICATING; CASE MATERIAL: CERAMIC; SPECIFICATION: DIN 43620; REFERENCE NO: 3NE4330; SLOT LENGTH 17MM X 10.5MM","EA",10]
[117615,"FUSE, CARTRIDGE: CURRENT: 500 A; POTENTIAL: 500 V; CONNECTION TYPE: BLADE KNIFE; DIMENSIONS: SQ 70 X LG 150 MM; TYPE: SLO BLO, INDICATING; CASE MATERIAL: CERAMIC; SPECIFICATION: VDE0636/2; SUPPL P/N: 3NA 1434; 3/GL-GI","EA",6]
[117616,"FUSE, CARTRIDGE: CURRENT: 250 A; POTENTIAL: 800 VAC; 500 VDC; DIMENSIONS: SQ 60 X LG 142 MM; TYPE: INDICATING; CASE MATERIAL: CERAMIC; SPECIFICATION: IEC 269; VDE 0636; REFERENCE NO: 3NE4327; 3NE4327-OB","EA",10]
[117617,"FUSE, CARTRIDGE: CURRENT: 315 A; POTENTIAL: 500 VAC; CONNECTION TYPE: BLADE KNIFE; DIMENSIONS: WD 53 X LG 149 X HT 59 MM; TYPE: INDICATING; CASE MATERIAL: CERAMIC; REFERENCE NO: 3NA3252","EA",75]
[117633,"FUSE, CARTRIDGE: CURRENT: 20 A; POTENTIAL: 32 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 6.4 X LG 32 MM; TYPE: FAST BLOW; CASE MATERIAL: GLASS; AUTO, ONE TIME","EA",10]
[117634,"FUSE, CARTRIDGE: CURRENT: 15 A; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 6.4 X LG 32 MM; TYPE: FAST BLOW; CASE MATERIAL: GLASS; REFERENCE NO: 13215; AUTOMOBILE, TUBE, 6.3MM DIAMETER, ONE TIME","EA",10]
[117635,"FUSE, CARTRIDGE: CURRENT: 25 A; POTENTIAL: 500 V; TYPE: FAST BLOW; SPECIFICATION: DIN 49515; VDE 0635; SUPPL P/N: 5SB181; DIAZED, SUITABLE FOR E27 THREAD BASE, QIUCK RESPONSE","EA",10]
[117641,"FUSE, CARTRIDGE: CURRENT: 100 A; POTENTIAL: 415-550 VAC; 460 VDC; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 36 X LG 108 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; SPECIFICATION: BS 88-1975; REFERENCE NO: TCP100; A4; LOW VOLTAGE HRC, CATEGOTY OF DUTY 550AC80, BS DIA, FIX CENTRES 94 MM","EA",794]
[117643,"FUSE, CARTRIDGE: CURRENT: 63 A; POTENTIAL: 660 VAC; CONNECTION TYPE: BLADE KNIFE; DIMENSIONS: WD 30 X LG 77 X HT 47 MM; TYPE: INDICATING; CASE MATERIAL: CERAMIC; SUPPL P/N: 3NE8 018; TEF 2020920/63","EA",10]
[117644,"FUSE, CARTRIDGE: CURRENT: 6 A; POTENTIAL: 500 VAC; CONNECTION TYPE: BLADE KNIFE; DIMENSIONS: WD 20 X LG 78 X HT 40 MM; TYPE: INDICATING; CASE MATERIAL: CERAMIC; SUPPL P/N: 3NA3801","EA",277]
[117714,"FUSE, CARTRIDGE: CURRENT: 50 A; POTENTIAL: 500 VAC; CONNECTION TYPE: FERRULE; DIMENSIONS: WD 40 X LG 78 X HT 20 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; SUPPL P/N: 3NA3820","EA",139]
[117733,"FUSE, CARTRIDGE: CURRENT: 5 A; POTENTIAL: 500 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 22 X LG 50 MM; TYPE: INDICATING; CASE MATERIAL: CERAMIC; SUPPL P/N: EL1621504; ORIGINAL DIAZED, FOR USE ON LP SERVICES, ICE COMPRESSORS","EA",10]
[117750,"FUSE, CARTRIDGE: CURRENT: 63 A; POTENTIAL: 500 VAC; CONNECTION TYPE: BLADE KNIFE; DIMENSIONS: WD 20 X LG 78 X HT 36 MM; TYPE: INDICATING; CASE MATERIAL: CERAMIC; SUPPL P/N: 3NA3822; TEF 2000013/63","EA",102]
[117751,"FUSE, CARTRIDGE: CURRENT: 32 A; POTENTIAL: 500 V; CONNECTION TYPE: BLADE; DIMENSIONS: WD 40 X LG 85 X HT 22 MM; TYPE: FAST BLOW; CASE MATERIAL: CERAMIC; SUPPL P/N: 3NA3812","EA",400]
[117752,"FUSE, CARTRIDGE: CURRENT: 20 A; POTENTIAL: 500 V; CONNECTION TYPE: BLADE KNIFE; DIMENSIONS: WD 20 X LG 78 X HT 36 MM; TYPE: INDICATING; CASE MATERIAL: CERAMIC; SUPPL P/N: 3NA3807","EA",268]
[117753,"FUSE, CARTRIDGE: CURRENT: 10 A; POTENTIAL: 500 VAC; CONNECTION TYPE: BLADE KNIFE; DIMENSIONS: WD 20 X LG 78 X HT 36 MM; TYPE: INDICATING; CASE MATERIAL: CERAMIC; REFERENCE NO: 3NA3803","EA",35]
[117754,"FUSE, CARTRIDGE: CURRENT: 16 A; POTENTIAL: 500 VAC; CONNECTION TYPE: BLADE KNIFE; DIMENSIONS: WD 20 X LG 78 X HT 36 MM; TYPE: INDICATING; CASE MATERIAL: CERAMIC; SUPPL P/N: 3NA3805","EA",156]
[117759,"FUSE, CARTRIDGE: CURRENT: 25 A; POTENTIAL: 500 VAC; CONNECTION TYPE: BLADE KNIFE; DIMENSIONS: WD 21 X LG 79 X HT 40 MM; TYPE: INDICATING; CASE MATERIAL: CERAMIC; SUPPL P/N: 3NA3810","EA",147]
[117762,"FUSE, CARTRIDGE: CURRENT: 355 A; POTENTIAL: 500 VAC; DIMENSIONS: SQ 75 X LG 150 MM; TYPE: INDICATING; CASE MATERIAL: CERAMIC; SUPPL P/N: 3NA3254","EA",10]
[117780,"FUSE, CARTRIDGE: CURRENT: 25 A; POTENTIAL: 415 VAC; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 25 X LG 36 MM; TYPE: SLO BLO, INDICATING; CASE MATERIAL: CERAMIC; SPECIFICATION: DIN 49522; REFERENCE NO: 5SE2025; NEOZED, OPERATION CLASS GL TO VDE, DIMENSIONS D02","EA",10]
[117781,"FUSE, CARTRIDGE: CURRENT: 6 A; POTENTIAL: 415 VAC; TYPE: SLO BLO; SPECIFICATION: DIN 49522; SUPPL P/N: 5SE2006; NEOZED, OPERATION CLASS GL TO VDE","EA",20]
[117786,"FUSE, CARTRIDGE: CURRENT: 80 A; POTENTIAL: 500 VAC; CONNECTION TYPE: SCREW CLAMP OFFSET TAGS; DIMENSIONS: DIA 31 X LG 135 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; SPECIFICATION: BS 88-1975; REFERENCE NO: A4; 3NWTCP80; LOW VOLTAGE HRC, BASE TYPE C, CLASS Q1","EA",5]
[117794,"FUSE, CARTRIDGE: CURRENT: 30 A; POTENTIAL: 500 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 14 X LG 50 MM; TYPE: FAST BLOW; CASE MATERIAL: CERAMIC; REFERENCE NO: A50P30; TYPE 1, 150 DEG C MAX","EA",10]
[117853,"FUSE, CARTRIDGE: CURRENT: 355 A; POTENTIAL: 3.6 KV; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 76.5 X LG 360 MM; TYPE: INDICATING; CASE MATERIAL: CERAMIC; HIGH VOLTAGE HRC, TYPE WKLAJ355A, STRIKER PIN 3LF562","EA",10]
[117854,"FUSE, CARTRIDGE: CURRENT: 8 A; POTENTIAL: 250 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 6.3 X LG 32 MM; TYPE: MINIATURE, FAST BLOW; CASE MATERIAL: CERAMIC; CURRENT LIMITING; GLASS TUBE","EA",10]
[117855,"FUSE, CARTRIDGE: CURRENT: 5 A; POTENTIAL: 250 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 6.3 X LG 32 MM; TYPE: FAST BLOW; CASE MATERIAL: PORCELAIN; REFERENCE NO: 059-0112; THYRISTOR CONTROL PANEL FOR INLINE HEATERS","EA",10]
[117856,"FUSE, CARTRIDGE: CURRENT: 1 A; POTENTIAL: 250 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 6.5 X LG 33 MM; TYPE: MINIATURE ANTI SURGE; CASE MATERIAL: GLASS; REFERENCE NO: TDC11","EA",10]
[117857,"FUSE, CARTRIDGE: CURRENT: 25 A; POTENTIAL: 32 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 6 X LG 26 MM; TYPE: MINIATURE, FAST BLOW; CASE MATERIAL: GLASS","EA",80]
[117858,"FUSE, CARTRIDGE: CURRENT: 4 A; POTENTIAL: 250 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 5 X LG 20 MM; TYPE: SLO BLOW; CASE MATERIAL: GLASS","EA",10]
[117859,"FUSE, CARTRIDGE: CURRENT: 15 A; POTENTIAL: 550 VAC; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 22 X LG 84 MM; INTERRUPT CAPACITY: 40 KA; TYPE: INDICATING; CASE MATERIAL: CERAMIC; SPECIFICATION: SABS 172-1977; REFERENCE NO: 5000101/16A; CLASS Q1, BEARING THE SABS MARK OF APPROVAL","EA",10]
[117860,"FUSE, CARTRIDGE: CURRENT: 16 A; POTENTIAL: 500 VAC; DIMENSIONS: DIA 10 X LG 38 MM; TYPE: TIME DELAY; CASE MATERIAL: CERAMIC; REFERENCE NO: TRM15; CURRENT RATING 15 AMP, 10000 SC, CURRENT LIMITING; GOULD SHAWNUTTRI-ONICS","EA",15]
[117861,"FUSE, CARTRIDGE: CURRENT: 20 A; POTENTIAL: 500 VAC; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 14 X LG 51 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: FIBER; CAT NO: A50P20 TYPE 1; REFERENCE NO: A50P20 TYPE 1","EA",15]
[117862,"FUSE, CARTRIDGE: CURRENT: 100 A; POTENTIAL: 500 VAC; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 22 X LG 58 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; SPECIFICATION: IEC 269/2; SUPPL P/N: SIBA-4008210","EA",15]
[117863,"FUSE, CARTRIDGE: CURRENT: 25 A; POTENTIAL: 11-12 KV; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 60 X LG 250 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; OEFMA 3GN 722","EA",21]
[117864,"FUSE, CARTRIDGE: CURRENT: 50 A; POTENTIAL: 7.2-12 KV; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 64 X LG 255 MM; TYPE: INDICATING; CASE MATERIAL: CERAMIC; SPECIFICATION: BS 2692; SUPPL P/N: KEBX0; 250MVA FREE AIR RATING","EA",10]
[117865,"FUSE, CARTRIDGE: CURRENT: 315 A; POTENTIAL: 3.3-3.6 KV; CONNECTION TYPE: SCREW CLAMP OFFSET; DIMENSIONS: DIA 76 X LG 360 MM; TYPE: INDICATING; CASE MATERIAL: CERAMIC; SUPPL P/N: 3NV915; WKFH5 -315A; HIGH VOLTAGE, HRC, TYPE LEL","EA",10]
[117866,"FUSE, CARTRIDGE: CURRENT: 160 A; POTENTIAL: 500 V; CONNECTION TYPE: BLADE KNIFE; DIMENSIONS: DIA 40 X LG 124 MM; TYPE: INDICATING; CASE MATERIAL: CERAMIC; REFERENCE NO: L83408; TO NORME 63211","EA",10]
[117874,"FUSE, CARTRIDGE: CURRENT: 25 A; POTENTIAL: 24 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 6.3 X LG 25 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: GLASS; AUTOMOBILE","EA",10]
[117907,"FUSE, CARTRIDGE: POTENTIAL: 11 KV; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 25.3 X LG 195 MM; INTERRUPT CAPACITY: 52.5 KA; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; FUSEGEAR CT, HRC","EA",10]
[117976,"FUSE, CARTRIDGE: CURRENT: 16 A; POTENTIAL: 415 VAC; TYPE: SLO BLO; SPECIFICATION: DIN 49522; SUPPL P/N: 5SE2016; NEOZED, OPERATION CLASS GL, TO VDE","EA",24]
[117997,"FUSE, CARTRIDGE: CURRENT: 20 A; POTENTIAL: 500 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 22 X LG 50 MM; TYPE: FAST BLOW INDICATING; CASE MATERIAL: CERAMIC; SPECIFICATION: DIN 49515; VDE 0635; REFERENCE NO: 5SB171; DIAZED, SUITABLE FOR E27 THREAD BASE, CHARACTERISTIC, QIUCK RESPONSE","EA",10]
[118002,"FUSE, CARTRIDGE: CURRENT: 63 A; POTENTIAL: 415-440 VAC; CONNECTION TYPE: KNIFE BLADE TAGS; DIMENSIONS: DIA 17.5 X LG 67 MM; INTERRUPT CAPACITY: 80 KA; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; SPECIFICATION: BS 88-1975 Q1; REFERENCE NO: 3NWES63; LOW VOLTAGE HRC, LABEL COLOUR CODE PURPLE, BASE TYPE E, CLASS Q1","EA",10]
[118004,"FUSE, CARTRIDGE: CURRENT: 32 A; POTENTIAL: 600 VAC; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 14 X LG 51 MM; TYPE: RAPID ULTRA INDICATING; CASE MATERIAL: CERAMIC; REFERENCE NO: 50-059-06; LOW VOLTAGE, HRC, STRIKER PIN ON ONE SIDE","EA",33]
[118065,"FUSE, CARTRIDGE: CURRENT: 6 A; POTENTIAL: 415 V; CONNECTION TYPE: BLADE KNIFE; DIMENSIONS: DIA 14 X LG 60 MM; TYPE: FAST BLOW; CASE MATERIAL: CERAMIC; SUPPL P/N: 5008601/6; NS6 HRC","EA",295]
[118068,"FUSE, CARTRIDGE: CURRENT: 50 A; POTENTIAL: 550-660 V; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 22 X LG 84 MM; INTERRUPT CAPACITY: 50 KA; TYPE: FAST BLOW; CASE MATERIAL: CERAMIC; SUPPL P/N: TCP; HRC, FOR USE ON CT CUBICLE FANS","EA",97]
[118069,"FUSE, CARTRIDGE: CURRENT: 355 A; POTENTIAL: 550 V; CONNECTION TYPE: CENTER SCREW CLAMP TAG; DIMENSIONS: DIA 55 X LG 200 MM; TYPE: FAST BLOW; CASE MATERIAL: CERAMIC; SUPPL P/N: 5003901/355; HRC, CLASS 1, 4 HOLE FIXING","EA",101]
[118105,"FUSE, CARTRIDGE: CURRENT: 10 A; POTENTIAL: 415 V; TYPE: LINK; CASE MATERIAL: CERAMIC","EA",20]
[118106,"FUSE, CARTRIDGE: CURRENT: 2 A; POTENTIAL: 415 V; CONNECTION TYPE: BLADE KNIFE; TYPE: INDICATING BOTTLE; CASE MATERIAL: CERAMIC; NEOZED","EA",10]
[118107,"FUSE, CARTRIDGE: CURRENT: 35 A; POTENTIAL: 400 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 13 X LG 35 MM; TYPE: SLO BLO, BOTTLE, INDICATING; CASE MATERIAL: CERAMIC; REFERENCE NO: 35A; 400/250 AMP, LINDNER GL, NEOZED","EA",20]
[118110,"FUSE, CARTRIDGE: CURRENT: 25 A; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 6 X LG 25 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: PLASTIC; OUTOMOBILE","EA",10]
[118139,"FUSE, CARTRIDGE: CURRENT: 2 A; POTENTIAL: 415 VAC; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 13 X LG 54 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: GLASS; SUPPL P/N: NIT2; SUPPLIER NOTE, THE ITEM MUST BE PROTECTIVE PACKED AND CLEARLY MARKED","EA",80]
[118146,"FUSE, CARTRIDGE: CURRENT: 10 A; POTENTIAL: 550 VAC; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 13 X LG 54 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; SUPPL P/N: NIT10; SUPPLIER NOTE, THE ITEM MUST BE PROTECTIVE PACKED AND CLEARLY MARKED","EA",148]
[118158,"FUSE, CARTRIDGE: CURRENT: 25 A; POTENTIAL: 500 VAC; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 14 X LG 50 MM; TYPE: FAST BLOW INDICATING; CASE MATERIAL: CERAMIC; REFERENCE NO: 5SA181; DIAZED","EA",15]
[118159,"FUSE, CARTRIDGE: CURRENT: 25 A; POTENTIAL: 500 VAC; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 22 X LG 50 MM; TYPE: FAST BLOW INDICATING; CASE MATERIAL: CERAMIC; SPECIFICATION: DIN 49515; SUPPL P/N: 5SB181; REFERENCE NO: VDE0635; DIAZED, SUITABLE FOR E27 THREAD BASE, QUICK RESPONSE","EA",10]
[118166,"FUSE, CARTRIDGE: CURRENT: 32 A; POTENTIAL: 600 VAC; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 14 X LG 51 MM; TYPE: FAST BLOW INDICATING; CASE MATERIAL: CERAMIC; SUPPL P/N: 621CPURE14-32; NORMAL INSTANTANEOUS OPERATING, 14MM DIAMETER HOLE, ONE TIME","EA",10]
[118168,"FUSE, CARTRIDGE: CURRENT: 40 A; POTENTIAL: 415 VAC; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 22 X LG 85 MM; INTERRUPT CAPACITY: 80 KA; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; SPECIFICATION: BS 88 IEC 60269; SUPPL P/N: TIS40; BS 88 OR IEC 60 269 CERTIFIED; FUSE BODY LENGTH 56.4 MM; BREAKING RANGE AND UTILIZATION CATEGORY: GG; SIZE: A3; SUPPLIER NOTE, THE ITEM MUST BE PROTECTIVE PACKED AND CLEARLY MARKED","EA",290]
[118197,"FUSE, CARTRIDGE: CURRENT: 400 A; POTENTIAL: 500 VAC; CONNECTION TYPE: BLADE KNIFE; DIMENSIONS: SQ 57 X LG 150 MM; TYPE: INDICATING; CASE MATERIAL: CERAMIC; SUPPL P/N: 3NA3260; FUSE, CARTRIDGE; CURRENT 400 A, POTENTIAL 500 VAC, DIMENSIONS SQ 57 X LG 150 MM, TYPE INDICATING, CASE MATERIAL CERAMIC, CONNECTION TYPE BLADE KNIFE, PART NUMBER: 3NA3260~FUSE,CARTD;3NA3260,400 A,500 VAC","EA",10]
[118211,"FUSE, CARTRIDGE: CURRENT: 1 A; POTENTIAL: 250 VAC; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 5 X LG 20 MM; TYPE: FAST BLOW; CASE MATERIAL: GLASS; REFERENCE NO: T1-250; TRANSPARENT BODIED OR WINDOW TYPE","EA",10]
[118223,"FUSE, CARTRIDGE: CURRENT: 350 A; POTENTIAL: 130 VAC; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 25 X LG 68 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: FIBER; REFERENCE NO: A13X350","EA",10]
[118224,"FUSE, CARTRIDGE: CURRENT: 450 A; POTENTIAL: 550 VAC; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 75 X LG 210 MM; TYPE: FAST BLOW; CASE MATERIAL: CERAMIC; SUPPL P/N: TTM450","EA",10]
[118235,"FUSE, CARTRIDGE: CURRENT: 10 A; POTENTIAL: 500 VAC; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 14 X LG 51 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: PORCELAIN; REFERENCE NO: S25","EA",10]
[118239,"FUSE, CARTRIDGE: CURRENT: 63 A; POTENTIAL: 550 V; CONNECTION TYPE: SCREW CLAMP CENTER TAGS; DIMENSIONS: DIA 26.2 X LG 128.7 MM; TYPE: INDICATING; CASE MATERIAL: CERAMIC; MODEL NO: TBC 63; HRC, OR APPROVED EQUIVALENT, 8.70MM W SLOT, 111MM MTG CENTERS, ONE TIME, HOLE BLOWN IN LABLE","EA",139]
[118266,"FUSE, CARTRIDGE: CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 7.5 X LG 45 MM; TYPE: TRIP INDICATING; CASE MATERIAL: CERAMIC; SUPPL P/N: GS700; REFERENCE NO: T1300; SUPPLIER NOTE, THE ITEM MUST BE PROTECTIVE PACKED AND CLEARLY MARKED","EA",10]
[118272,"FUSE, CARTRIDGE: CURRENT: 50 A; POTENTIAL: 240 VAC; CONNECTION TYPE: SCREW CLAMP OFFSET TAGS; DIMENSIONS: DIA 17 X LG 55 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC","EA",15]
[118274,"FUSE, CARTRIDGE: CURRENT: 63 A; POTENTIAL: 500-550 VAC; CONNECTION TYPE: BLADE KNIFE; DIMENSIONS: DIA 21.4 X LG 90.5 MM; TYPE: INDICATING; CASE MATERIAL: CERAMIC; SPECIFICATION: BS 88 PART 1; CAT NO: A3; CLASS Q1, LIST NO 13163","EA",10]
[118276,"FUSE, CARTRIDGE: CURRENT: 75 A; POTENTIAL: 660 VAC; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 16 X LG 78 MM; TYPE: INSTANTANEOUS; CASE MATERIAL: CERAMIC; SUPPL P/N: GSB75; REFERENCE NO: 5007306/75A; HRC, NORMAL OPERATING, OFFSET AXIAL LUG TYPE 6.4 MM, W SLOT 63.2 MM MTG CENTERS, ONE TIME, NON INDICATING","EA",10]
[118284,"FUSE, CARTRIDGE: CURRENT: 160 A; POTENTIAL: 500 VAC; CONNECTION TYPE: BLADE KNIFE; DIMENSIONS: WD 49 X LG 135 X HT 44 MM; INTERRUPT CAPACITY: 120 KA; TYPE: SLO BLO, INDICATING; CASE MATERIAL: CERAMIC; SUPPL P/N: 20003 13; NH1 GL GG","EA",51]
[118288,"FUSE, CARTRIDGE: CURRENT: 630 A; POTENTIAL: 500 VAC; CONNECTION TYPE: BLADE KNIFE; DIMENSIONS: WD 70 X LG 150 X HT 79 MM; TYPE: INDICATING; CASE MATERIAL: CERAMIC; SUPPL P/N: 3NA3372","EA",10]
[118303,"FUSE, CARTRIDGE: CURRENT: 250 MA; POTENTIAL: 250 VAC; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 5 X LG 20 MM; TYPE: FAST BLOW; CASE MATERIAL: GLASS; SUPPL P/N: 5 X 20","EA",500]
[118304,"FUSE, CARTRIDGE: CURRENT: 0.5 A; POTENTIAL: 250 VAC; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 5 X LG 20 MM; TYPE: TIME DELAY SLO BLO; CASE MATERIAL: GLASS; REFERENCE NO: 19195; T0-5-250","EA",80]
[118306,"FUSE, CARTRIDGE: CURRENT: 2 A; POTENTIAL: 250 VAC; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 6 X LG 30 MM; TYPE: INDICATING; CASE MATERIAL: GLASS; REFERENCE NO: BUSSGL02; SPRING LOADED","EA",10]
[118309,"FUSE, CARTRIDGE: CURRENT: 2 A; POTENTIAL: 500 VAC; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 10 X LG 38 MM; TYPE: FAST BLOW; CASE MATERIAL: CERAMIC; REFERENCE NO: C63210; TYPE GL","EA",10]
[118316,"FUSE, CARTRIDGE: CURRENT: 4 A; POTENTIAL: 250 VAC; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 5 X LG 20 MM; TYPE: MEDIUM TIME LAG; CASE MATERIAL: GLASS; SUPPL P/N: 520.623; CURRENT LIMITING; ONE TIME, NON INDICATING, ESKA","EA",10]
[118327,"FUSE, CARTRIDGE: CURRENT: 16 A; POTENTIAL: 415 VAC; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 10 X LG 36.5 MM; TYPE: BOTTLE INDICATING; CASE MATERIAL: CERAMIC; SUPPL P/N: 5SE2016; NEOZED","EA",10]
["0118338","FUSE, CARTRIDGE: CURRENT: 32 A; POTENTIAL: 660 VAC; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 22 X LG 58 MM; TYPE: INDICATING; CASE MATERIAL: CERAMIC; REFERENCE NO: 621CPURE22-32; FOR USE ON ASH STACKING SYSTEM","EA",10]
[118345,"FUSE, CARTRIDGE: CURRENT: 50 A; POTENTIAL: 600 VAC; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 22 X LG 58 MM; TYPE: INDICATING; CASE MATERIAL: CERAMIC; REFERENCE NO: 621CP URE; 22-32, PIN EXTENDS FROM END","EA",50]
[118359,"FUSE, CARTRIDGE: CURRENT: 160 A; POTENTIAL: 3.3-3.6 KV; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 68 X LG 255 MM; TYPE: INDICATING; CASE MATERIAL: CERAMIC; HIGH VOLTAGE, COMPLETE WITH STRIKER PIN INDICATION, LEL, TYPE OEFMA","EA",10]
[118362,"FUSE, CARTRIDGE: CURRENT: 250 A; POTENTIAL: 600 VAC; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 34.6 X LG 106.4 MM; TYPE: FAST BLOW; CASE MATERIAL: CERAMIC; SUPPL P/N: GSB250","EA",3]
[118364,"FUSE, CARTRIDGE: CURRENT: 250 A; POTENTIAL: 3.3-3.6 KV; CONNECTION TYPE: LUG AXIAL OFFSET SCREW CLAMP; DIMENSIONS: DIA 76 X LG 336.55 MM; TYPE: INSTANTANEOUS INDICATING; CASE MATERIAL: CERAMIC; REFERENCE NO: WKFHO; HRC LEL, COMPLETE WITH STRIKER PIN; NORMAL OPERATING, 10MM WIDE SLOT, 31.75 X 304MM CENTERS, ONE TIME, PIN EXTENDS FROM END","EA",10]
[118367,"FUSE, CARTRIDGE: CURRENT: 350 A; POTENTIAL: 200 V; CONNECTION TYPE: LUG AXIAL OFFSET SCREW CLAMP; DIMENSIONS: DIA 34.6 X LG 85 MM; INTERRUPT CAPACITY: 100 KA; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; SUPPL P/N: GSD350; HRC, 10.3MM WIDE SLOT, 60.3MM MOUNTING CENTRE, ONE TIME","EA",10]
[118369,"FUSE, CARTRIDGE: CURRENT: 350 A; POTENTIAL: 3.3 KVAC; CONNECTION TYPE: SCREW CLAMP OFFSET TAGS; DIMENSIONS: DIA 80 X LG 340 MM; TYPE: INDICATING; CASE MATERIAL: CERAMIC; SUPPL P/N: K81PEX350A; TYPE AKFHO, COMPLETE WITH STRIKER PIN INDICATOR , LEL","EA",10]
[118434,"FUSE, CARTRIDGE: CURRENT: 500 MA; POTENTIAL: 250 VAC; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 5 X LG 20 MM; TYPE: SLO BLO, MINIATURE; CASE MATERIAL: GLASS; REFERENCE NO: M0-5-250C; CURRENT LIMITING; TYPE CEB","EA",110]
[118438,"FUSE, CARTRIDGE: CURRENT: 4 A; POTENTIAL: 250 VAC; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 5 X LG 25 MM; TYPE: INDICATING; CASE MATERIAL: CERAMIC; REFERENCE NO: M4-250G; COLOURED BEAD EXTENDS FROM ONE END","EA",10]
[118441,"FUSE, CARTRIDGE: CURRENT: 6 A; POTENTIAL: 415 VAC; 250 VDC; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 10 X LG 36 MM; TYPE: BOTTLE INDICATING; CASE MATERIAL: CERAMIC; SUPPL P/N: D01; REFERENCE NO: 5SE2006; NEOZED","EA",10]
[118444,"FUSE, CARTRIDGE: CURRENT: 10 A; POTENTIAL: 415-500 VAC; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 10 X LG 36 MM; TYPE: SLO BLO, INDICATING; CASE MATERIAL: CERAMIC; SPECIFICATION: DIN 49 522; REFERENCE NO: 5SE2010; NEOZED, OPERATION CLASS GL TO VDE","EA",50]
[118461,"FUSE, CARTRIDGE: CURRENT: 125 A; POTENTIAL: 500 VAC; CONNECTION TYPE: BLADE KNIFE; DIMENSIONS: WD 48 X LG 78 X HT 20 MM; TYPE: SLO BLO, INDICATING; CASE MATERIAL: CERAMIC; SPECIFICATION: DIN 43620; VDE 0636/21; REFERENCE NO: 3NA4832; LINK, CLASS GL","EA",345]
[118481,"FUSE, CARTRIDGE: CURRENT: 32 A; POTENTIAL: 415 VAC; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 22 X LG 84 MM; INTERRUPT CAPACITY: 80 KA; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; SPECIFICATION: BS 88 IEC 60269; SUPPL P/N: TIA32; HRCFUSE BODY LENGTH: 56.4 MM; BREAKING RANGE AND UTILIZATION CATEGORY: GG; SIZE: A2","EA",930]
[118497,"FUSE, CARTRIDGE: CURRENT: 80 A; POTENTIAL: 600 V; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 25 X LG 112 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: FIBER; CAT NO: A60X80TYPE4; REFERENCE NO: A60X80","EA",30]
[118510,"FUSE, CARTRIDGE: CURRENT: 80 A; POTENTIAL: 500 VAC; CONNECTION TYPE: BLADE KNIFE; DIMENSIONS: WD 35 X LG 80 MM; TYPE: INDICATING; CASE MATERIAL: CERAMIC; SPECIFICATION: VDE0636; REFERENCE NO: 3NA4824; SIZE NH00C","EA",5]
[118512,"FUSE, CARTRIDGE: CURRENT: 100 A; POTENTIAL: 690 VAC; CONNECTION TYPE: BLADE KNIFE; DIMENSIONS: WD 30 X LG 80 MM; TYPE: ULTRA RAPID INDICATING; CASE MATERIAL: CERAMIC; SPECIFICATION: IEC 269; VDE 0636; SUPPL P/N: 2020920/100A; REFERENCE NO: 3NE8021","EA",483]
[118513,"FUSE, CARTRIDGE: CURRENT: 10 A; POTENTIAL: 415-550 VAC; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 14 X LG 54 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; REFERENCE NO: 5008501/10A","EA",85]
[118518,"FUSE, CARTRIDGE: CURRENT: 560 A; POTENTIAL: 550 V; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 75.5 X LG 207 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; SUPPL P/N: TTM560","EA",10]
[118983,"FUSE, CARTRIDGE: CURRENT: 4 A; POTENTIAL: 500 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 10 X LG 38 MM; TYPE: SLO BLO; CASE MATERIAL: PORCELAIN; REFERENCE NO: 133 04; CURRENT LIMITING; TYPE GL","EA",80]
[119008,"FUSE, CARTRIDGE: CURRENT: 10 A; POTENTIAL: 500 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 10 X LG 38 MM; TYPE: SLO BLO; CASE MATERIAL: PORCELAIN; REFERENCE NO: 133 10; CURRENT LIMITING; GL","EA",75]
[119101,"FUSE, CARTRIDGE: CURRENT: 3 A; POTENTIAL: 600 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 10 X LG 35 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC","EA",10]
[119131,"FUSE, CARTRIDGE: CURRENT: 90 A; POTENTIAL: 7.2-12 KV; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 64 X LG 355 MM; INTERRUPT CAPACITY: 40 KA; TYPE: INDICATING; CASE MATERIAL: CERAMIC; SPECIFICATION: BS 2692-1975; STRIKER PIN, TYPE KEMXO90A, FUSE GEAR, 20KA","EA",10]
[119133,"FUSE, CARTRIDGE: CURRENT: 250 A; POTENTIAL: 500 VAC; CONNECTION TYPE: BLADE KNIFE; DIMENSIONS: SQ 47 X LG 134 MM; INTERRUPT CAPACITY: 120 KA; TYPE: INDICATING; CASE MATERIAL: CERAMIC; SUPPL P/N: 2000313/250; 3NA4144","EA",178]
[119134,"FUSE, CARTRIDGE: CONNECTION TYPE: BOLTED; DIMENSIONS: DIA 40.4 X LG 134 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; REFERENCE NO: S2110-399; ENGLISH ELECTRIC","EA",10]
[119139,"FUSE, CARTRIDGE: CURRENT: 50 A; POTENTIAL: 550 VAC; CONNECTION TYPE: SCREW CLAMP; DIMENSIONS: DIA 24 X LG 87 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; REFERENCE NO: 5000201; TIS50; CLASS Q1","EA",184]
[119181,"FUSE, CARTRIDGE: CURRENT: 25 A; POTENTIAL: 400 VAC; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 10 X LG 38 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; SUPPL P/N: AM25","EA",30]
[119182,"FUSE, CARTRIDGE: CURRENT: 32 A; POTENTIAL: 380 VAC; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 10 X LG 38 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; REFERENCE NO: GF32; 4006232; IFO","EA",90]
[119183,"FUSE, CARTRIDGE: CURRENT: 1.6 A; POTENTIAL: 250 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 5 X LG 20 MM; TYPE: MINIATURE, FAST BLOW; CASE MATERIAL: GLASS","EA",30]
[119184,"FUSE, CARTRIDGE: CURRENT: 315 A; POTENTIAL: 250 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 5 X LG 25 MM; TYPE: MINIATURE, FAST BLOW; CASE MATERIAL: GLASS","EA",10]
[119185,"FUSE, CARTRIDGE: CURRENT: 800 MA; POTENTIAL: 250 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 5 X LG 20 MM; TYPE: MINIATURE, FAST BLOW; CASE MATERIAL: GLASS; TUBE","EA",911]
[119186,"FUSE, CARTRIDGE: CURRENT: 1 A; POTENTIAL: 250 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 6 X LG 25 MM; TYPE: FAST BLOW; CASE MATERIAL: GLASS","EA",10]
[119187,"FUSE, CARTRIDGE: CURRENT: 1.25 A; POTENTIAL: 250 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 6.3 X LG 25 MM; TYPE: MINIATURE, FAST BLOW; CASE MATERIAL: GLASS","EA",30]
[119188,"FUSE, CARTRIDGE: CURRENT: 1.6 A; POTENTIAL: 125-250 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 6.3 X LG 25 MM; TYPE: MINIATURE, FAST BLOW; CASE MATERIAL: GLASS","EA",10]
[119189,"FUSE, CARTRIDGE: CURRENT: 2 A; POTENTIAL: 250 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 6.3 X LG 25 MM; TYPE: MINIATURE, FAST BLOW; CASE MATERIAL: GLASS; SPECIFICATION: ISO 9001","EA",10]
[119190,"FUSE, CARTRIDGE: CURRENT: 2.5 A; POTENTIAL: 125 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 6 X LG 25 MM; TYPE: FAST BLOW; CASE MATERIAL: GLASS","EA",10]
[119191,"FUSE, CARTRIDGE: CURRENT: 5 A; POTENTIAL: 250 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 6.3 X LG 25 MM; TYPE: MINIATURE, FAST BLOW; CASE MATERIAL: GLASS","EA",10]
[119192,"FUSE, CARTRIDGE: CURRENT: 160 A; POTENTIAL: 250 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 5 X LG 20 MM; TYPE: MINIATURE, FAST BLOW; CASE MATERIAL: GLASS","EA",10]
[119194,"FUSE, CARTRIDGE: CURRENT: 800 MA; POTENTIAL: 250 V; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 5 X LG 25 MM; TYPE: FAST BLOW; CASE MATERIAL: GLASS","EA",136]
[119209,"FUSE, CARTRIDGE: CONNECTION TYPE: BOLTED; DIMENSIONS: DIA 34 X LG 137 MM; TYPE: INDICATING; CASE MATERIAL: CERAMIC; MODEL NO: S2147","EA",8]
[119558,"FUSE, CARTRIDGE: CURRENT: 1 A; POTENTIAL: 3.6-7.2 KV; CONNECTION TYPE: FERRULE; DIMENSIONS: DIA 22 X LG 194 MM; TYPE: VTDNN; CASE MATERIAL: CERAMIC; SUPPL P/N: B6780; VTDNN; 12 KV, FOR USE ON ASH STACKER","EA",10]
[210336,"FUSE, CARTRIDGE: CURRENT: 32 A; POTENTIAL: 415 VAC; INTERRUPT CAPACITY: 80 KA; TYPE: COMPACT DIMENSION FUSE LINKS; SPECIFICATION: BS 88; IEC 60269-2; SUPPL P/N: NS32A; CLASS CARTRIDGE, LAWSON CLIPFIT, DUAL FOR CURRENT/TIME LIMITOR, ON DELIVERY A TEST CERTIFICATE FOR RECOVERY VOLTAGE","EA",30]
[210602,"FUSE, CARTRIDGE: CURRENT: 32 A; POTENTIAL: 415 VAC; CASE MATERIAL: GLASS; SPECIFICATION: IEC 60269-2; SUPPL P/N: NS32A; CONNECTION BS88","EA",20]
[220812,"FUSE, CARTRIDGE: CURRENT: 4 A; POTENTIAL: 550 VAC; CONNECTION TYPE: BLADE; DIMENSIONS: DIA 10 X LG 32 MM; TYPE: OFFSET; CASE MATERIAL: CERAMIC; SUPPL P/N: A87721/93/59","EA",5]
[222661,"FUSE, CARTRIDGE: CURRENT: 10 A; POTENTIAL: 550 V; CONNECTION TYPE: BLADE; DIMENSIONS: DIA 10 X LG 35 MM; CASE MATERIAL: CERAMIC; SUPPL P/N: 10 FOG; REFERENCE NO: A87721/93/60; FOR USE ON STACKER","EA",21]
[222662,"FUSE, CARTRIDGE: CURRENT: 25 A; POTENTIAL: 11 KV; CONNECTION TYPE: PUSH IN; DIMENSIONS: DIA 62 X LG 254 MM; TYPE: CURRENT LIMITING; CASE MATERIAL: CERAMIC; SUPPL P/N: OEFMA; FOR USE ON STACKER","EA",10]
[222664,"FUSE, CARTRIDGE: CURRENT: 315 A; POTENTIAL: 600 V; CONNECTION TYPE: STUD; DIMENSIONS: SQ 40 MM; TYPE: DC PANEL; CASE MATERIAL: CERAMIC; REFERENCE NO: A87721/93/3; FOR USE ON STACKER","EA",190]
[222665,"FUSE, CARTRIDGE: CURRENT: 125 A; POTENTIAL: 600 V; CONNECTION TYPE: STUD; DIMENSIONS: WD 102 X LG 143 MM; TYPE: SLEW DC; CASE MATERIAL: CERAMIC; SUPPL P/N: J8996; FOR USE ON STACKER","EA",251]
[222666,"FUSE, CARTRIDGE: CURRENT: 4 A; POTENTIAL: 600 V; CONNECTION TYPE: CAP; DIMENSIONS: DIA 10 X LG 37 MM; TYPE: PANEL; CASE MATERIAL: CERAMIC; REFERENCE NO: A87721/93/58; FOR USE ON STACKER","EA",10]