{"text_format":"3","workbook":"xls","n_sheets":12,"sheets":["1. Preliminary and General","2. QC & A","3. H & S","4. Environmental","5. Civil - Site Clearance","6. Civil - Concrete","7. Civil - Structural Steel","8. Civil - Struct Stl-corrosion","9. Mechanical","10. Electrical","11. Automation","12.Summary"],"not_rendered":{"images":12,"external_links":1,"defined_names":11},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"1. Preliminary and General","index":0,"n_rows":210,"n_cols":7,"rows_kept":210,"merged":[[1,7,2,7],[50,0,50,2],[52,0,52,5],[89,0,89,2],[91,0,91,5],[148,0,148,2],[150,0,150,5],[207,0,207,2],[209,0,209,5]],"flags":["formulas_cached_only"]}
[null,null,"Zuikerbosch Pumping Station: ",{"$nulls":3},"SANS 1200A"]
[null,null,"Polyelectrolyte Dosing Plant 2 @ WA1",{"$nulls":3},"Section 1 :  Preliminary & General Costs"]
[]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate","Amount"]
[]
[1,"SANS 1200A","SECTION 1:  GENERAL (SMALL WORKS)"]
[1.1,8.3,"SCHEDULED FIXED-CHARGE AND VALUE-RELATED ITEMS"]
["1.1.1","8.3.1","Contractual Requirements","Sum",1]
["1.1.2","8.3.2","Provision of facilities on site"]
["1.1.2.1",null,"a) Facilities required by Engineer"]
[null,"PSAB 3.2 PSAB 5.2","        Provision of Office for the Engineer's \n        Representative ","Sum",1]
[]
[null,null,"        4 Covered parking bays as directed by the \n        Engineer","Sum",1]
[]
[null,null,"        Construction name boards x 2","Sum",1]
[]
["1.1.2.2",null,"b) Facilities required by Contractor"]
[null,null,"        Offices, storage sheds, fencing, workshops, \n        laboratories, etc.","Sum",1]
[]
[null,null,"        Ablution and latrine facilities","Sum",1]
[]
[null,null,"        Tools and equipment","Sum",1]
[]
[null,null,"        Water supplies, electric power and \n        communications","Sum",1]
[]
[null,null,"        Other fixed charge obligations, including \n        setting out of works, security of contractor's \n        plant & personnel","Sum",1]
[]
[null,null,"        Remove all site establishment on completion","Sum",1]
[]
[null,null,"        Security of Contractor's plant","Sum",1]
[]
["1.2",8.7,"Provision for Health and Safety Measures (Fixed Charge)"]
[]
["1.2.1",null,"i) Preparation and submission of the contractor's site specific health and safety plan","Sum",1]
[]
["1.2.2",null,"ii) Provision of personal protective equipment (PPE)","Sum",1]
[]
["1.2.3",null,"iii) Cost of medical certificates and medical surveillance","Sum",1]
[]
["1.2.4",null,"iv) Other Items not listed above ","Sum",1]
[]
["1.3",8.8,"Provision for Enviroment Measures (Fixed Charge)"]
[]
["1.3.1",null,"i) Pollution prevention","Sum",1]
[]
["1.3.2",null,"ii) Waste disposal provision","Sum",1]
[]
["1.3.3",null,"iii) Administration and documentation","Sum",1]
[]
[]
["Total Carried forward ",{"$nulls":5},0]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate","Amount"]
["Total  brought Forward  "]
[]
["1.4",8.4,"TIME RELATED CHARGES"]
[]
["1.4.1","8.4.1","Contractual Requirements","Sum",1]
[]
["1.4.2","8.4.2.","Operation and maintenance of facilities on site"]
[]
["1.4.2.1",null,"a) Facilities for engineer","Sum",1]
[]
["1.4.2.2",null,"b) Facilities for contractor","Sum",1]
[]
["1.4.3","8.4.3","General responsibilities and other time-related obligations","Sum",1]
[]
["1.5",8.5,"Temporary Works"]
[]
["1.5.1","8.5.1","Access to works including all temporary roads, ramps, excavations and reinstatement of road/s etc.","Sum",1]
[]
["1.6",8.6,"SINGLE ITEM SCHEDULED"]
[]
["1.6.1",null,"Accomodation of Traffic"]
[]
["1.6.1.1",null,"ii) The supply, maintaining and removal of traffic control devices, road signs, chanalisation of traffic, barricades, warning signs, including signs for construction vehicles and road markings","Sum",1]
[]
["1.6.2",null,"Temporary Storage Shed"]
[]
["1.6.2.1",null,"iv) The sum shall cover the Contractor's cost to erect a storage shed for the temporary storage (for the duration of the Contract) of dismantled steel and concrete elements (dismanted during the construction process). The shed shall protect the stored items against all incident weather that is expected to occur during construction. The rate shall also include the cost of designing and submitting the design of the shed to the Engineer for approval - shed is expected to be at least 150m2 in plan and 3m high, cladded with IBR Sheet on 100x100x8 Portal frames spaced at around 4m)","Sum",1]
[]
["1.7",8.7,"Provision for Health and Safety Measures (Time Related)"]
[]
["1.7.1",null,"i) Safety officer on site","Sum",1]
[]
["1.7.2",null,"ii) Cost of medical certificates and medical surveillance","Sum",1]
[]
["1.7.3",null,"iii) Detection of existing services","Sum",1]
[]
["1.7.4",null,"iv) Other Items not listed above (To be qualified)","Sum",1]
["Total Carried forward "]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate","Amount"]
["Total Brought Forward  "]
[1.18,"SABS 1200A","\nTIME RELATED ITEMS"]
[]
["1.18.1","8.4.1","Contractual Requirements","Sum",1]
[]
["1.18.1.1","8.4.2","Operate and maintain facilities on Site"]
[]
["1.18.2","8.4.2","Facilities for Engineer for duration of Contract (SABS 1200AB)"]
[]
["1.18.2.1","PSAB 3.2 PSAB 5.2","Provision of office for the Engineer's representative","Sum",1]
[]
["1.18.2.2","PSAB 4.2","Provision of survey equipment","Sum",1]
[]
["1.18.2.3","8.3.2.1(b)","4 Covered parking bays as directed by the Engineer","Sum",1]
[]
["1.18.2.4","8.4.2.1(c)","Name Board as shown on Sketch bound to back of document","Sum",1]
[]
["1.18.2.5","8.4.2.1(d)","Provision of survey assistants","Sum",1]
[]
["1.18.3","8.4.2.2","Facilities for Contractor"]
[]
["1.18.3.1","8.4.2.2\n(a)(b)(c)","Offices, storage sheds, fencing, workshops, laboratories, etc.","Sum",1]
[]
["1.18.3.2","8.4.2.2(e)","Ablution and latrine facilities","Sum",1]
[]
["1.18.3.3","8.4.2.2(f)","Tools and equipment","Sum",1]
[]
["1.18.3.4","8.4.2.2(g)","Water supplies, electric power and communications","Sum",1]
[]
[1.19,"PSA 8.8.7","Dealing with water","Sum",1]
[]
[{"v":1.2,"d":"1.20"},"8.4.3","Supervision for duration of construction","Sum",1]
[]
[1.21,"8.4.4","Company and head office overhead costs","Sum",1]
[]
[1.22,"8.4.5","Other time related charges, including security of contractor's plant & personnel","Sum",1]
[]
[1.23,null,"Accommodation of traffic"]
[]
["1.23.1","PSA 8.8.2  and 8.6 (k)    ","The supply, maintaining and removal of traffic control devices, road signs, canalisation of traffic, barricades, including New Jersey type, warning signs, including signs for construction vehicles and road markings","Sum",1]
[]
[1.24,null,"As Builts"]
[]
["1.24.1","PSA 8.16","The provision of detailed as-builts drawings of the completed works","Sum",1]
[]
[1.25,null,"Access to Spoil Sites"]
[]
["1.25.1","PS 17","Sum associated with identification, negotiations and access to designated spoil sites for disposal of surplus spoil material","Sum",1]
[]
[1.26,null,"Temporary Works"]
[]
["1.26.1","8.8.1","Access to works including all temporary roads, excavations and ramps, etc.","Sum",1]
[]
[1.27,null,"Other costs"]
[]
["1.27.1","PSA 8.8.8","Discontinue operations (where instructed by the Engineer due to lack of access) and transfer plant,equipement and labour"]
[]
["Total Carried forward "]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate","Amount"]
["Total Brought Forward  "]
[]
[1.27,null,"Other costs"]
[]
["1.27.1","PSA 8.8.8","Discontinue operations (where instructed by the Engineer due to lack of access) and transfer plant,equipement and labour"]
[]
["1.27.1.1",null,"De-establishing and Re-establishing after phase 1","Sum",1]
[]
["1.27.1.2",null,"De-establishing and Re-establishing after phase 2","Sum",1]
[]
["1.27.1.3",null,"De-establishing and Re-establishing after phase 3","Sum",1]
[]
[1.28,"PSA 8.8.11","Standing time costs ","Days",40]
[]
[1.29,"PSA 8.8.12","Carry out operations in a confined and reduced working strip width","m",200]
[]
[{"v":1.3,"d":"1.30"},"8.8.4","Existing services"]
[]
["1.31.1",null,"a) Supply or hire specialist equipment for the detection of underground services","Sum",1]
[]
["1.31.2",null,"b) The use of equipment referred to in item (a) above","Sum",1]
[]
["1.31.3",null,"c) Excavation by hand in soft material to expose services","Sum",1]
[]
["1.31.4",null,"d) Temporary protection","Sum",1]
[]
[1.32,"PSA 8.10","Provision of crane with about 50m arm reach for working above the Sasol Pipeline in order to protect it throughout the construction period of the header upgrading.","Sum",1]
{"$rows_empty":30}
["Total Carried forward "]
[]
["Total Section 1: Carried Forward to Summary"]

{"sheet":"2. QC & A","index":1,"n_rows":51,"n_cols":7,"rows_kept":51,"merged":[[49,0,49,2],[50,0,51,5],[50,6,51,6]],"flags":["formulas_cached_only"]}
[null,null,"Zuikerbosch Pumping Station: ",{"$nulls":3},"Section 2:  Quality Control and Assurance"]
["Contract No.:",null,"Polyelectrolyte Dosing Plant 2 @ WA1"]
["Description:"]
[]
["Item ","Payment","Description","Unit","Qty","Rate","Amount"]
["No.","Refers"]
[2,"PSA 8.3.14","SECTION 2:  QUALITY CONTROL AND ASSURANCE"]
[]
[2.1,null,"Preparation and submission of Contractors Quality Management Plan (CQMP), for review and approval prior to commencement of works","Sum",1]
[]
[2.2,null,"Implementing activities of the Quality Control Plan or Inspection Test Plan ","Sum",1]
[]
[2.3,null,"Provision of Qualified Quality Officer ( The contractor shall provide RW with relevant to the scope of work  qualified Quality Officer )","Sum",1]
[]
[2.4,null,"Maintenance of documents and final documentation for submission ","Sum"]
[]
[2.5,null,"Provision of Quality Officers relevant training ( The contractor to provide related training for the quality officer ) ",1,1]
[]
[2.6,null,"Provision of Compliance Audits ( The contractor to audit the project once a year for the duration of the project ) ",1,1]
[]
[2.7,null,"Testing Equipment calibration ( The testing Equipments should be calibrated as per the manual ) ","Sum",1]
[]
[2.8,null,"Welders qualification  training as per the code ( The contractors must qualify the welders as per API 5L ) ",1,1]
[]
[2.9,null,"Provision of any other  testing and inspections requested by the Engineer","Sum",1]
{"$rows_empty":24}
["Total brought forward "]
["Total Section 2: Carried Carried Forward to Summary"]

{"sheet":"3. H & S","index":2,"n_rows":110,"n_cols":7,"rows_kept":110,"merged":[[6,6,7,6],[109,0,109,5]],"flags":["formulas_cached_only"]}
[{"$nulls":6},"Section 3:  Occupational Health & Safety"]
["Contract No.:",null,"Zuikerbosch Pumping Station: "]
["Description:",null,"Polyelectrolyte Dosing Plant 2 @ WA1"]
[]
["Item ","Payment","Description","Unit","Qty","Rate","Amount"]
["No.","Refers"]
[null,null,"SECTION 3 :  OCCUPATIONAL HEALTH AND SAFETY "]
[]
[3.1,null,"Preparation of the Contractor's site specific Health and Safety Plan","  lump sum"]
[]
[3.2,null,"Principal Contractor's initial obligations in respect of the Occupational Health and Safety Act and Construction Regulations","  lump sum"]
[]
[3.3,null,"Principal Contractor's time related obligations in respect of the Occupational Health and Safety Act and Construction Regulations","  month"]
[]
[3.4,null,"Provision of Personal Protective Equipment (PPE)"]
[]
[3.5,null,"Provision of a full-time Construction Health and Safety Officer"," month"]
[]
[3.6,null,"Cost of medical certificates and medical surveillance"]
[]
[null,null,"(a) Initial (baseline) medical examinations","lump sum"]
[]
[null,null,"(b) Periodic  examinations","lump sum"]
[]
[null,null,"(c)Exit examinations","lump sum"]
[]
[3.7,null,"Induction training","lump sum"]
[]
[3.8,null,"Provision of First Aid Boxes to GSR requirements and other emergency safety equipment such as fire extinguishers.","lump sum"]
[]
[3.9,null,"Transportation of Workers","lump sum"]
[]
[{"v":3.1,"d":"3.10"},null,"Welfare Facilities","lump sum"]
[]
[3.11,null,"Occupational Hygiene Surveys","lump sum"]
[]
[3.12,null,"Training","lump sum"]
[]
[3.13,null,"Security requirements including the security risk assessment (before site establishment)","  lump sum"]
[]
[3.14,null,"Employee wellness programs","lump sum"]
[]
[3.15,null,"Drug and Alcohol Testing, Policies and Procedures","lump sum"]
[]
[3.16,null,"Barricading","lump sum"]
[]
[3.17,null,"Safety notices and signs","lump sum"]
[]
[3.18,null,"SHE  Incentives","lump sum"]
[]
[3.19,null,"COVID-19 Prevention and Management "]
[]
["3.19.1",null,"Preparation of the Contractor's site specific COVID Plan & Risk Assessment including the recording & reporting of COVID statistics","lump sum"]
[{"$nulls":3},"lump sum"]
["3.19.2",null,"COVID-19 related training and education","lump sum"]
[{"$nulls":3},"lump sum",2]
["3.19.3",null,"Non-Contact Digital Thermometer/calibrated","lump sum"]
[{"$nulls":3},"lump sum",4]
["3.19.4",null,"Foot Operated hand sanitiser stand ( adjustable for variuos bottles types - preferable the stand with signage \" sanitise hands here\" and 'Arrow \" by the foot). At entrance points to site camps and construction sites and at the works area","lump sum"]
[]
["3.19.5",null,"Hand Sanitiser Dispenser 600 ml ( Wall mounted)  - Automatic sensor (no touch) - suitable for liquid and gel sanitiser. At hot spots namely kitchen, ablution,by shared office equipment boardrooms etc.","lump sum"]
[]
["3.19.6",null,"Hand Soap Dispenser 600 ml ( Wall mounted)  - Automatic sensor (no touch). For the kitchen.","lump sum"]
[]
["3.19.7",null,"Empty Sanitiser spray bottles ( 500ml )","lump sum"]
[]
["3.19.8",null,"Water Container with Tap ( 25 Litre)","lump sum"]
[]
["3.19.9",null,"Bio-hazard bin for Covid-19 waste ( 100 L) ","lump sum"]
[]
["3.19.10",null,"Provision of no touch/pedal  refuse bins  ( 50 L) for kitchen, dining rooms, & boardrooms","lump sum"]
[]
["3.19.11",null,"Prefab Isolation Room near site camp entrance","lump sum"]
[]
["3.19.12",null,"Face Shield for screeners/tester(s)","lump sum"]
[]
["3.19.13",null,"Covid-19 Awareness Signage Posters/Notice at entrances/social distancing floor markings","lump sum"]
[]
["3.19.14",null,"Cloth masks ( 2 per employee)","Lump sum"]
[]
["3.19.15",null,"Batteries for Thermometer & Dispenser","Monthly"]
[]
["3.19.16",null,"Medical/Disinfectant ( Alcohol) -Wipes Canister (5L)","Monthly"]
[]
["3.19.17",null,"Full body Coverall with hood  for Screeners/testers ( 1 per day)","Monthly"]
[{"$nulls":4},4]
["3.19.18",null,"Examination Gloves for screeners/tester(s) ( Box of 100)","Monthly"]
[]
["3.19.19",null,"Screening stickers per day (Box of 250)","Monthly"]
[]
["3.19.20",null,"Surgical Masks for suspected/sick person(s) /Screeners/testers ( Box of 100)","Monthly"]
[]
["3.19.21",null,"Disinfection Control by Accredited proffesional services","Quarterly"]
[]
["3.19.22",null,"Disinfectant solutions for surface ( 5L)","Monthly"]
[]
["3.19.23",null,"Hand Sanitizers solution for refills ( 5 L)","Monthly"]
[]
["3.19.24",null,"Hand soap for refills (5L)","Monthly"]
[]
["3.19.25",null,"Personal Hand Sanitizer ( carry - 50ml)","Monthly"]
[]
["3.19.26",null,"Biological waste Skip Disposal","Monthly"]
[]
[{"v":3.2,"d":"3.20"},null,"Adequate ventilation and lighting during construction","lump sum"]
[]
[3.21,null,"Submission of the Health and Safety File (hard and soft copies)","lump sum"]
[]
[]
["Total Section 3:  Carried Forward to Summary"]

{"sheet":"4. Environmental","index":3,"n_rows":95,"n_cols":7,"rows_kept":95,"merged":[[45,0,45,2],[47,0,47,5],[94,0,94,5]],"flags":["formulas_cached_only"]}
[{"$nulls":6},"Section 4:  Environment"]
[null,null,"Zuikerbosch Pumping Station: "]
[null,null,"Polyelectrolyte Dosing Plant 2 @ WA1"]
[]
["Item ","Payment","Description","Unit","Qty","Rate","Amount"]
["No.","Refers"]
[null,"PSA 8.3.14","SECTION 4 :  ENVIRONMENT"]
[]
[4,null,"ENVIRONMENT"]
[]
[4.1,null,"Signage"]
[]
["4.1.1",null,"No go area","Sum",1]
[]
["4.1.2",null,"Environmental Sign at gate","Sum",1]
[]
[]
[4.2,null,"Pollution prevention"]
[]
["4.2.1",null,"Fire protection equipment. Two flappers (fire beaters) and one fire extinguisher per team","Sum",1]
[]
["4.2.2",null,"Waste bins and receptacles that comply with the waste clauses of the EMP (all types of waste and waste seperation to be catered for throughout the working area)","Sum",1]
[]
["4.2.3",null,"Adequate serviced ablution facilities as per EMP and OHS Act.","Sum",1]
[]
["4.2.4",null,"Designated eating and smoking areas as per EMP","Sum",1]
[]
["4.2.5",null,"Water cart/s  to adequately provide dust control of whole site (minimum of three times a day)","Sum",1]
[]
["4.2.6",null,"Spillage kits","Sum",1]
[]
["4.2.7",null,"Drip trays for all vehicles parked overnight ","Sum","as required"]
[]
["4.2.8",null,"Bunding facility for hazardous products as per OHS Act","Sum","as required"]
[]
["4.2.9",null,"Labeled containers for decanting of liquids.","Sum","as required"]
[]
[4.3,null,"Waste Removal to Registered Waste Facility as per EMP"]
[]
["4.3.1",null,"General waste","Sum",1]
[]
["4.3.2",null,"Hazardous waste","Sum",1]
[]
[]
[]
["Total brought forward "]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate","Amount"]
["Total Carried Forward  "]
[]
[4.4,null,"Erosion control, silt management and soil management"]
[]
["4.4.1",null,"Silt fences ","m",30]
[]
["4.4.2",null,"Hay bales (100m)","m",30]
[]
["4.4.3",null,"Sand bags (100m)","m",50]
[]
[4.5,null,"Administration and documentation"]
[]
["4.5.1",null,"Submission of Environmental File (For approval by Rand Water ECO)","Sum",1]
[]
["4.5.2",null,"Contractor's appointed Environmental Officer to have relevant training. ( Minimum of environmental law one week training from a reputable provider). The safety officer can have a dule function if he or she has the appropriate training.","Sum",1]
[]
["4.5.2",null,"Maintenance of Environmental file and final documentation for submission ","Sum",1]
{"$rows_empty":30}
["Section 4 :  Carried Forward to Summary"]

{"sheet":"5. Civil - Site Clearance","index":4,"n_rows":49,"n_cols":7,"rows_kept":49,"flags":["formulas_cached_only"]}
[null,null,"Zuikerbosch Pumping Station: ",{"$nulls":3},"SANS 1200C"]
[null,null,"Polyelectrolyte Dosing Plant 2 @ WA1",{"$nulls":3},"Section 5: Site Clearance"]
[]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No","Refers"]
[]
["5","SANS 2001 BS1","SECTION 5:  SITE CLEARANCE"]
[]
[null,"BS1-7","SCHEDULED ITEMS"]
[]
["5.1","8.2.8","Demolish and remove structures/buildings and dismantle steelworks","Sum",1]
[]
["5.1.1",null,"i) Demolish and remove existing concrete apron around the Poly electrolyte plant (as per DRG No. R023464/900)","Sum",1]
[]
["5.1.2",null,"ii) Structural Steelworks (frames for walkways, cat ladders, staircases and grating) as per drawing R023464/900 ","Sum",1]
{"$rows_empty":33}
[null,null,"Section 5 :Carried Forward to Summary",{"$nulls":3},0]

{"sheet":"6. Civil - Concrete","index":5,"n_rows":60,"n_cols":7,"rows_kept":60,"merged":[[57,0,57,2]],"flags":["formulas_cached_only"]}
[null,null,"Zuikerbosch Pumping Station: ",{"$nulls":3},"SANS 1200GA"]
[null,null,"Polyelectrolyte Dosing Plant 2 @ WA1",{"$nulls":3},"Section 6: Concrete"]
[]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No","Refers"]
[]
[6,"SANS\n2001 CC1","SECTION 6: CONCRETE WORKS (STRUCTURAL) "]
[]
[null,"CC1 - 6","MEASUREMENT AND PAYMENT"]
[]
[6.1,"8.2","SCHEDULED FORMWORK ITEMS"]
[null,null,"Supply all materials, install and remove formwork (rate to include for forming of 20 x 20 chamfers to all exposed edges for:)"]
[]
["6.1.1","8.2.3","Narrow Widths"]
[]
["6.1.1.1",null,"i) Sides of  column (350mm high) refer to DRG No. RA23464 and RA23465","m",9]
[]
["6.1.1.2",null,"ii) Sides of  column 250mm high) refer to DRG No. RA23464 and RA23465","m",12]
[]
[6.2,"8.3","SCHEDULED REINFORCEMENT ITEMS"]
[]
["6.2.1","8.3.1","Steel bars"]
[null,null,"For the concrete footings "]
[]
["6.2.1.1",null,"i) Mild steel reinforcement","Sum",1]
[]
["6.2.1.2",null,"ii) High tensile steel reinforcement","Sum",1]
[]
[6.3,8.4,"SCHEDULED CONCRETE ITEMS"]
[]
["6.3.1","8.4.3","Strength Concrete, Grade ..."]
[]
["6.3.1.1",null,"i) Grade 30MPa/19mm:","Sum",1]
[]
["6.3.2","8.4.4","Unformed Surface Finishes"]
[]
["6.3.2.1",null,"a) Wood-floated finish to top of footin and column","Sum",1]
[]
[6.4,8.7,"Grouting"]
[]
["6.4.1",null,"30Mpa Non-shrinking grout for the repair the walls with honeycomb ","m3",{"v":0.5,"d":"1"}]
[]
[]
[6.5,null,"Miscellaneous "]
[]
["6.5.1",null,"i) Concrete brickwork for the access steps (as per DRG No. R023464/901)","Sum",1]
{"$rows_empty":11}
["Total Carried Forward "]
[]
[null,null,"Section 6 :  Carried Forward to Summary",{"$nulls":3},0]

{"sheet":"7. Civil - Structural Steel","index":6,"n_rows":65,"n_cols":7,"rows_kept":65,"merged":[[44,0,44,2],[46,0,46,5]],"flags":["formulas_cached_only"]}
[null,null,"Zuikerbosch Pumping Station: ",{"$nulls":3},"SANS 1200HA"]
[null,null,"Polyelectrolyte Dosing Plant 2 @ WA1",{"$nulls":3},"Section 7: Structural steelwork"]
[]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No","Refers"]
[]
[7,"SANS 2001:CS1","SECTION 7: STRUCTURAL STEELWORK "]
[]
[null,"8.3","SCHEDULED ITEMS"]
[]
[7.1,"8.3.1","Supply and Fabrication"]
[]
["7.1.1","8.3.1.1","Preparation of shop detail drawings"]
[]
["7.1.2",null,"i) Structural Steelworks (frames for walkways, cat ladders and staircases - excluding grating) as per drawing R023464/900 ","t",9.5]
[]
[null,"8.3.1.2","Supply and fabrication of steelwork"]
[]
[null,null,"i) Structural Steelworks (frames for walkways, cat ladders and staircases - excluding grating) as per drawing R023464/900","t",9.5]
[]
[null,"8.3.2","Delivery to Site"]
[]
[null,"8.3.2.1.","Normal Delivery"]
[]
[null,null,"i) Structural Steelworks (frames for walkways, cat ladders and staircases - excluding grating) as per drawing R023464/900 ","t",9.5]
[]
[null,"8.3.3","Erection on Site"]
[]
[null,null,"i) Structural Steelworks (frames for walkways, cat ladders and staircases - excluding grating) as per drawing R023464/900 ","t",9.5]
[]
[null,"8.3.6","Holding Down Bolts"]
[]
[null,null,"i) Structural Steelworks (frames for walkways, cat ladders and staircases - excluding grating) as per drawing R023464/900 ","Sum",1]
[]
[null,"8.3.7","Handrails"]
[]
[null,null,"a) Handrails assembly complete (as per DRG No. R023464/900 and R023465/200&201)","Sum",1]
[]
[null,"8.3.8 ","Ladders, complete and intalled as per DRG No. R023464/900"]
[]
[null,null,"i) 1m high Fibre Reinforced Polymer catladder","No.",1]
[null,null,"i) 2.4m high steel catladder","No.",1]
[]
[]
["Total Carried Forward "]
["Item  No. ","Payment Refers ","Description","Unit","Qty","Rate","Amount"]
["Total  brought Forward  "]
[]
[null,"8.3.9","Flooring, Complete and Installed with frames"]
[]
[null,null,"a) Open grid floors"]
[]
[null,null,"i) RS 40x4.5 steel grating (as per DRG No. R023464/900)","m2",12]
[]
[null,null,"ii) Fibre Reinforced Polymer grating (as per DRG No. R023464/900&901)","m2",105]
[]
[null,"8.3.10","Non-destructive Testing"]
[]
[null,null,"i) Structural Steelworks (frames for walkways, cat ladders and staircases - excluding grating) as per drawing R023464/900 ","Sum",1]
[{"$nulls":6},0]
[null,"8.3.12","Additional Items"]
[]
[null,null,"i) Additional steel bolts, gusset plates and members required for the construction and erection of steel and FRP elements - the rate should include the manufacture, corrosion protection (by galvanizations as per the project specification), delivery, and installation of all steel elements","Sum",1]
[]
[null,null,"Section 7 :  Carried Forward to Summary",{"$nulls":3},0]

{"sheet":"8. Civil - Struct Stl-corrosion","index":7,"n_rows":47,"n_cols":7,"rows_kept":47,"merged":[[44,0,44,2]],"flags":["formulas_cached_only"]}
[null,null,"Zuikerbosch Pumping Station: ",{"$nulls":3},"SANS 1200HC"]
[null,null,"Polyelectrolyte Dosing Plant 2 @ WA1",{"$nulls":3},"Section 8: Corrosion Protection of Structural Steelwork"]
[]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No","Refers"]
[]
[8,"SANS 1200HC","SECTION 8: CORROSION PROTECTION OF STRUCTURAL STEELWORK"]
[]
[null,null,"All structural steel to be Hot Dipped Galvanized to the requirements of SANS 763"]
[]
[8.1,8.2,"SCHEDULED ITEMS"]
[]
["8.1.1","8.2.1","Surface Dressing and Repairs at Place of Fabrication"]
[]
["8.1.1.1",null,"i) Structural Steelworks (frames for walkways, cat ladders and staircases - excluding grating) as per drawing R023464/900 ","Sum",1]
[]
["8.1.2","8.2.2","Transport"]
[]
["8.1.2.1",null,"i) Structural Steelworks (frames for walkways, cat ladders and staircases - excluding grating) as per drawing R023464/900 ","Sum",1]
[]
["8.1.3","8.2.3","Surface Preparation and Coating Application"]
[]
["8.1.3.1",null,"a) in the shop"]
[]
[null,null,"i) Structural Steelworks (frames for walkways, cat ladders and staircases - excluding grating) as per drawing R023464/900 ","Sum",1]
{"$rows_empty":19}
["Total Carried Forward "]
[]
[null,null,"Section 8 :  Carried Forward to Summary",{"$nulls":3},0]

{"sheet":"9. Mechanical","index":8,"n_rows":298,"n_cols":9,"rows_kept":298,"merged":[[0,1,0,2],[3,0,3,6],[6,0,6,6],[62,0,62,2],[64,0,64,5],[65,0,66,6],[105,0,105,2],[108,0,108,5],[160,0,160,2],[163,0,163,5],[164,0,165,6],[219,0,219,2],[222,0,222,5],[297,0,297,5]],"flags":["formulas_cached_only"]}
[null,"Zuikerbosch Pumping Station: ",{"$nulls":4},"Section 9:  Mechanical"]
[null,"Polyelectrolyte Dosing Plant 2 @ WA1"]
[]
["SECTION 9:  MECHANICAL DESIGN, SUPPLY, DELIVERY AND INSTALLATION"]
["ITEM NUMBER","DESCRIPTION","UNIT","QUANTITY","REF","RATE","AMOUNT"]
[9,"Please refer to the Mechanical Engineering specification details and Drawings in order to price for below items. The Contractor’s responsibilities under this project include, but are not limited to, the following items:"]
["9.1 DEMOLITION WORK (REMOVAL)"]
["9.1.1","Offloading area"]
[]
["9.1.1.1","90  OD Class 12 PVC offloading pipeline","length","5m"]
["9.1.1.2","90 OD Class 12 PVC tank inlet pipeline","Length","26m"]
["9.1.1.3","90 OD Class 12 PVCtank inlet pipeline","Length","21m"]
["9.1.1.4","90 OD Class 12 PVC tank inlet pipeline","Length","17m"]
["9.1.1.5","90 OD Class 12 PVC tank inlet pipeline","Length","17m"]
["9.1.1.6","90 OD Class 12 PVC tan inlet pipeline","Length","26m"]
["9.1.1.7","90 OD Class 12 PVC tank inlet pipeline","Length","21m"]
["9.1.1.8","Manual ball valve ","Item",1,"RA 29069-001"]
["9.1.1.9","Non return valve","Item",1,"RA 29069-001"]
["9.1.1.10","Y type strainer","item",1,"RA 29069-001"]
["9.1.1.11","manual ball valve","item ",6,"RA 29069-001"]
["9.1.1.12","manual ball valve 25 OD PVC drain valve","item",2,"RA 29069-001"]
[]
["9.1.2","Top of bund"]
[]
["9.1.2.1","Drain manual ball valve for the tanks","Item",6]
["9.1.2.2","Tank outlet ball valves","Item",6]
["9.1.2.3","Actuated ball valve","Item",6]
["9.1.2.4","Isolation ball valve","Item",12]
["9.1.2.5","110 OD PVC pipeline","Length","10m"]
["9.1.2.6","Drain manual ball valve for the tank outlet line","Item",6]
["9.1.2.7","Strainer inlet and outlet manual ball valves","Item",8]
["9.1.2.8","Flow totalizer","Item",2]
["9.1.2.9","Manual isolation valve","Item",4]
["9.1.2.10","Manual isolation valves","Item",16]
["9.1.2.11","Magnetic level gauges","Item",6]
["9.1.2.12","110 OD Class 12 PVC tank outlet pipeline","Length","8m"]
["9.1.2.13","110 OD Class 12 PVC tank outlet pipeline","Length","12m"]
["9.1.2.14","110 OD Class 12 PVC tank outlet pipeline","Length","18m"]
["9.1.2.15","110 OD Class 12 PVC tank outlet pipeline","Length","8m"]
["9.1.2.16","110 OD Class 12 PVC tank outlet pipeline","Length","12m"]
["9.1.2.17","110 OD Class 12 PVC tank outlet pipeline","Length","17m"]
[null," "]
[]
["9.1.3","Pump room"]
[]
["9.1.3.1","Pump inlet actuated ball valve","Item",16]
["9.1.3.2","Non return valve","Item",32]
["9.1.3.3","Manual isolation valve","Item",16]
["9.1.3.4","Manual isolation valve for  calibration vessel","Item",16]
["9.1.3.5","Calibration vessel","Item",8]
["9.1.3.6","Pump with flexible hose","Item",16]
["9.1.3.7","Magnetic flow meter","Item",16]
["9.1.3.8","Pressure relief valve","Item",16]
["9.1.3.9","Pressure indication transmitter","Item",16]
["9.1.3.10","Manual ball valve","Item",16]
["9.1.3.11","Non return valve","Item",16]
["9.1.3.12","Actuated ball valve for the water line","Item",16]
["9.1.3.13","Magnetic flow meter for the water ine","Item",16]
["9.1.3.14","Non return valve","Item",16,{"$nulls":4}," "]
["9.1.3.15","32 OD PVC pipeline","Length","120m"]
["9.1.3.16","75 OD PVC pipeline","Length","120m"]
[]
["Total Carried Forward "]
["ITEM NUMBER","DESCRIPTION","UNIT","QUANTITY","REF","RATE","AMOUNT"]
["Total  brought Forward  "]
["9.2. SUPPLY"]
[]
["9.2.1","Foyer Area"]
["9.2.1.1","A water supply line complete with isolation valve and other accessories for washing the truck bay area connected at the available point as per design.","Set",1,"SS 4.2.5"]
[]
["9.2.2","MCC Room"]
["9.2.2.1","Painting for UPS support all round, including the area where the UPS is sitting.","Area","57m2"]
["9.2.3","Pump Room"]
[]
["9.2.3.1","New carbon steel carriage water pipe line DN 100 SCH 40 CS","Length","13m","SS 4.2.5              RA39 693/16"]
["9.2.3.2","New 100 NB 90°  bend CS","Item",5,"RA 39693/16"]
["9.2.3.3","100 NB - 80 NB reducer CS","Item",2,"RA 39693/16"]
["9.2.3.4","New 80 NB 90°  bend CS","Item",2,"RA 39693/16"]
["9.2.3.5","80 NB CS SCH 40 Pipe","Length","0.4m","RA 39693/16"]
["9.2.3.6","100 NB flanged isolation valve","Item",2,"RA 39693/16"]
["9.2.3.7","80 NB end flange","Item",1,"RA 39693/16"]
["9.2.3.8"," New Anchor bolts and bolt down all the pump-benches where the bolts are missing. Use similar bolts for this job. M12 x 100","Item",12]
["9.2.3.9","New 32 NB 90°  bend PVC","Item",260,"SS 4.2.5"]
["9.2.3.10"," New  3 litre calibration vessel ","Item",8,"SS 4.2.5"]
["9.2.3.11"," New 32 OD PVC actuated Ball valve","Item",4,"SS 4.2.4"]
["9.2.3.12","New 75 OD PVC actuated ball valve","Item",4,"SS 4.2.4"]
["9.2.3.13","New 75 OD Class 16 PVC pipeline","Length",1,"SS 4.2.5"]
["9.2.3.14","  New 32 OD Class 16 PVC pipeline","Length",1,"SS 4.2.5"]
["2.3.15"," New 75 NB 90°  bend PVC","Item",160,"SS 4.2.5"]
["9.2.3.16","New stubs for all demolished  manual valves 32 OD","Item",96,"RA 29069"]
["9.2.3.17","New stubs for all demolished actuated valves 75 OD","Item",32,"RA 29069"]
["9.2.3.18","New stubs for all demolished actuated valves 32 OD","Item",32,"RA 29069"]
["9.2.3.19","New stubs for all demolished non return valves 32 OD","Item",96,"RA 29069"]
["9.2.3.20","New stubs for all demolished non return valves 75 OD","Item",32,"RA 29069"]
["9.2.3.21","Unequal  Tee fitting for 75 OD and 32 OD pipes","Item",80,"RA 29069"]
["9.2.3.22","New  threaded connectors for pressure relief valve on 32 OD PVC pipe","Item",32,"RA 29069"]
["9.2.3.23","New 32 NB 45°  bend PVC for pressure instrument","Item",32,"RA 29069"]
["9.2.3.24","Tee fitting for 32 OD pipe","Item",112,"RA 29069"]
["9.2.3.25","New 32 OD Manual ball valve","Item",6]
["9.2.3.26","New 32 OD PVC threaded connectors","Item",16]
["9.2.3.27","New  75 OD PVC threaded connectors","Item",16]
["9.2.3.28","75 OD Class 12 HDPE pipeline","Length","30m"]
["9.2.3.29","75 OD HDPE Tee fitting ","Item",16]
["9.2.3.30","Reducing bush for 75OD HDPE to 32 OD PVC","Item",16]
[]
["Total Carried Forward "]
[]
["ITEM NUMBER","DESCRIPTION","UNIT","QUANTITY","REF","RATE","AMOUNT"]
["Total  brought Forward  "]
["9.2.4","Top Bund"]
["9.2.4.1"," 110 OD Class 12 HDPE tank outlet pipeline","Length","10m","RA 39693/07"]
["9.2.4.2"," 110 OD Class 12 HDPE tank outlet pipeline","Length","15m","RA 39693/08"]
["9.2.4.3"," 110 OD Class 12 HDPE tank outlet pipeline","Length","22m","RA 39693/09"]
["9.2.4.4"," 110 OD Class 12 HDPE tank outlet pipeline","Length","10m","RA 39693/10"]
["9.2.4.5"," 110 OD Class 12 HDPE tank outlet pipeline","Length","15m","RA 39693/11"]
["9.2.4.6"," 110 OD Class 12 HDPE tank outlet pipeline","Length","21m","RA 39693/12"]
["9.2.4.7","90 OD Class 12 HDPE tank inlet pipeline","Length","31m","RA 39693/01"]
["9.2.4.8","90 OD Class 12 HDPE tank inlet pipeline","Length","25m","RA 39693/02"]
["9.2.4.9","90 OD Class 12 HDPE tank inlet pipeline","Length","22m","RA 39693/03"]
["9.2.4.10","90 OD Class 12 HDPE tank inlet pipeline","Length","21m","RA 39693/04"]
["9.2.4.11","90 OD Class 12 HDPE tank inlet pipeline","Length","21m","RA 39693/05"]
["9.2.4.12","90 OD Class 12 HDPE tank inlet pipeline","Length","33m","RA 39693/06"]
["9.2.4.13","110 NB 90° bend HDPE","Item",24,"SS 4.2.5"]
["9.2.4.14","90 NB 90°  bend HDPE","Item",64,"SS 4.2.5"]
["9.2.4.15","110 NB 45° adjustable elbow","Item",15,"SS 4.2.5"]
["9.2.4.16","90 NB 45° adjustable elbow","Item",15,"SS 4.2.5"]
["9.2.4.17","25 OD Class 12 HDPE drain pipe","Length","1m","SS 4.2.5"]
["9.2.4.18","Gaskets NB 90","Item",12,"SS 4.2.5"]
["9.2.4.19","Gaskets NB 110","Item",53,"RA 39693"]
["9.2.4.20"," 110 NB HDPE adapter complete with stainless steel backing ring","Item",60,"SS 4.2.5"]
["9.2.4.21","90 NB HDPE adapter complete with stainless steel backing ring","Item",60,"SS 4.2.5"]
["9.2.4.22","Water supply line complete with isolation valve  and accessories for washing the roof area connected at the available point as per design.","Set",1,"SS 4.2.5"]
["9.2.4.23","Stubs for 25 OD manual ball valve","Item",12]
[]
["9.2.5","Outside The Building/Poly Plant"]
["9.2.5.1","Top sump valve  (DN 150 CS)","Item",1,"SS 4.2.4"]
["9.2.5.2","Sump valve pipe line 150 OD HDPE","Length","3m"]
["9.2.5.3","  DN 15 Polyproplene with Teflon seating air relief valves for the strainers.","Item",2,"MIR10016509812"]
["9.2.5.4","Carriage water valves to water manifold (DN100 CS)","Items",2,"SS 4.2.4"]
["9.2.5.5"," Ball manual valve that feed the Polyelectolyte suction manifold (100 OD CS ball valve)","Item",1,"SS 4.2.4"]
["9.2.5.6","Sump  non contact Ultrasonic level gauge","item",1,"SS 4.3.7        SS 4.4.4",null," "]
[]
["9.2.6","Dosing Lines"]
["9.2.6.1","Labeling for all the dosing lines to show their destination and pump (either stand-by or duty, e.g. Duty - System A, or Stand-by System A)","SUM",1]
["9.2.6.2"," colour coding for all pipes to Rand Water specifications at regular intervals to be advised (e.g. every 5m)","SUM",1]
[]
["9.2.7","Outside Area(Miscellaneous)"]
["9.2.7.1","All bolts and nuts must be consistent, and place all missing bolts, nuts or washers.","Sum",1]
["9.2.7.2","Camlock fitting","Items",6]
["9.2.7.3","Unequal Tee fitting 75 x 32","Item",20,"SS 4.2.5"]
["9.2.7.4","Provide for WKS numbering tags for all equipment and instruments","SUM",1,"SS 4.2.5"]
["9.2.7.5"," U bolts for 75OD pipe","Item",500]
["9.2.7.6","\n140 IPE (2200mm high)","Item",4]
["9.2.7.7","(200 x 200 x 8 ) baseplate","Item",4]
["9.2.7.8"," M14 RAWL BOLTS\n","Item",20]
["9.2.7.9","Pipe clamps for 90 OD HDPE pipe\n","Item",28]
["9.2.7.10","CAT-AND-Mouse level gauge on all tanks","Item",6,"BAL10026493513 SS 4.2.1"]
["9.2.7.11","Validation and Update of P&ID and all other associated Drawings (Process, Civil, Architecture, Mechanical, Electrical and Automation) to indicate the true reflection of the installation and finalising these to \"AS BUILT” Status. ","Sum",1]
["9.2.7.12","Handing over to Rand Water ALL nonreusable items  removed from the existing plant for storage","Sum",1]
[]
["Total Carried Forward "]
[]
["ITEM NUMBER","DESCRIPTION","UNIT","QUANTITY","REF","RATE","AMOUNT"]
["Total  brought Forward  "]
["9.3. INSTALLATION"]
[]
["9.3.1","Offloading area"]
["9.3.1.1","Water supply line complete with isolation valve and other accessories for washing the truck bay area connected at the available point as per design.","SUM",1,"SS 4.2.5"]
["9.3.1.2","90  OD Class 12 PVC offloading pipeline","length","5m"]
["9.3.1.3","90 OD Class 12 PVC tank inlet pipeline","Length","26m","RA 39693/01"]
["9.3.1.4","90 OD Class 12 PVCtank inlet pipeline","Length","21m","RA 39693/02"]
["9.3.1.5","90 OD Class 12 PVC tank inlet pipeline","Length","17m","RA 39693/03"]
["9.3.1.6","90 OD Class 12 PVC tank inlet pipeline","Length","17m","RA 39693/04"]
["9.3.1.7","90 OD Class 12 PVC tan inlet pipeline","Length","17m","RA 39693/06"]
["9.3.1.8","90 OD Class 12 PVC tank inlet pipeline","Length","27m","RA 39693/01"]
["9.3.1.9","Manual ball valve ","Item",1,"RA 29069-001"]
["9.3.1.10","Non return valve","Item",1,"RA 29069-001"]
["9.3.1.11","Y type strainer","item",1,"RA 29069-001"]
["9.3.1.12","manual ball valve","item ",6,"RA 29069-001"]
["9.3.1.13","manual ball valve 25 OD PVC drain valve","item",2,"RA 29069-001"]
[]
["9.3.2","MCC Room"]
["9.3.2.1","UPS support to be painted all round, including the area where the UPS is sitting.","Area","57m2"]
[]
["9.3.3","Pump Room"]
["9.3.3.1","New carbon steel carriage water pipe line DN 100 SCH 40 CS","Length","13m","SS 4.2.5              RA39 693/16"]
["9.3.3.2","New 100 NB 90°  bend CS","Item",5,"RA 39693/16"]
["9.3.3.3","100 NB - 80 NB reducer CS","Item",2,"RA 39693/16"]
["9.3.3.4","New 80 NB 90°  bend CS","Item",2,"RA 39693/16"]
["9.3.3.5","80 NB CS SCH 40 Pipe","Length","0.4m","RA 39693/16"]
["9.3.3.6","100 NB flanged isolation valve","Item",2,"RA 39693/16"]
["9.3.3.7","80 NB end flange","Item",1,"RA 39693/16"]
["9.3.3.8"," New Anchor bolts and bolt down all the pump-benches where the bolts are missing. Use similar bolts for this job. M12 x 100","Item",12]
["9.3.3.9","New 32 NB 90°  bend PVC","Item",260,"SS 4.2.5"]
["9.3.3.10"," New 3 litre calibration vessel","Item",8,"SS 4.2.5"]
["9.3.3.11"," New 32 OD PVC actuated Ball valve","Item",4,"SS 4.2.4"]
["9.3.3.12","New 75 OD PVC actuated ball valve","Item",4,"SS 4.2.4"]
["9.3.3.13","New 75 OD Class 16 PVC pipeline","Length","120m","SS 4.2.5"]
["9.3.3.14","  New 32 OD Class 16 PVC pipeline","Length","120m","SS 4.2.5"]
["9.3.3.15"," New 75 NB 90°  bend PVC","Item",160,"SS 4.2.5"]
["9.3.3.16","New stubs for all demolished  manual valves 32 OD","Item",96,"RA 29069"]
["9.3.3.17","New stubs for all demolished actuated valves 75 OD","Item",32,"RA 29069"]
["9.3.3.18","New stubs for all demolished actuated valves 32 OD","Item",32,"RA 29069"]
["9.3.3.19","New stubs for all demolished non return valves 32 OD","Item",96,"RA 29069"]
["9.3.3.20","New stubs for all demolished non return valves 75 OD","Item",32,"RA 29069"]
["9.3.3.21","Unequal  Tee fitting for 75 OD and 32 OD pipes","Item",80,"RA 29069"]
["9.3.3.22","New threaded connectors for pressure relief valve","Item",32,"RA 29069"]
["9.3.3.23","New 32 NB 45°  bend PVC for pressure instrument","Item",32,"RA 29069"]
["9.3.3.24","Tee fitting for 32 OD pipe","Item",112,"RA 29069"]
["9.3.3.25","New 32 OD Manual ball valve","Item",6]
["9.3.3.26","New 32 OD PVC threaded connectors","Item",16]
["9.3.3.27","New  75 OD PVC threaded connectors","Item",16]
["9.3.3.28","75 OD Class 12 HDPE pipeline","Length","30m"]
["9.3.3.29","75 OD HDPE Tee fitting ","Item",16]
["9.3.3.30","Reducing bush for 75OD HDPE to 32 OD PVC","Item",16]
["9.3.3.31"]
["9.3.3.32","Existing pump inlet actuated ball valve","Item",16]
["9.3.3.33","Existing non return valve","Item",32]
["9.3.3.34","Existing manual isolation valve","Item",16]
["Total Carried Forward "]
[]
["ITEM NUMBER","DESCRIPTION","UNIT","QUANTITY","REF","RATE","AMOUNT"]
["Total  brought Forward  "]
["9.3.3.35","Existing manual isolation valve for  calibration vessel","Item",16]
["9.3.3.36","Existing pump with flexible hose","Item",16]
["9.3.3.37","Existing magnetic flow meter","Item",16]
["9.3.3.38","Existing pressure relief valve","Item",16]
["9.3.3.39","Existing pressure indication transmitter","Item",16]
["9.3.3.40","Existing manual ball valve","Item",16]
["9.3.3.41","Existing non return valve","Item",16]
["9.3.3.42","Existing actuated ball valve for the water line","Item",16]
["9.3.3.43","Existing magnetic flow meter for the water ine","Item",16]
["9.3.3.44","Existing non return valve","Item",16]
[]
["9.3.4","Top bund"]
["9.3.4.1"," 110 OD Class 12 HDPE tank outlet pipeline","Length","10m","RA 39693/07"]
["9.3.4.2"," 110 OD Class 12 HDPE tank outlet pipeline","Length","15m","RA 39693/08"]
["9.3.4.3"," 110 OD Class 12 HDPE tank outlet pipeline","Length","22m","RA 39693/09"]
["9.3.4.4"," 110 OD Class 12 HDPE tank outlet pipeline","Length","10m","RA 39693/10"]
["9.3.4.5"," 110 OD Class 12 HDPE tank outlet pipeline","Length","15m","RA 39693/11"]
["9.3.4.6"," 110 OD Class 12 HDPE tank outlet pipeline","Length","21m","RA 39693/12"]
["9.3.4.7","90 OD Class 12 HDPE tank inlet pipeline","Length","31m","RA 39693/01"]
["9.3.4.8","90 OD Class 12 HDPE tank inlet pipeline","Length","25m","RA 39693/02"]
["9.3.4.9","90 OD Class 12 HDPE tank inlet pipeline","Length","22m","RA 39693/03"]
["9.3.4.10","90 OD Class 12 HDPE tank inlet pipeline","Length","21m","RA 39693/04"]
["9.3.4.11","90 OD Class 12 HDPE tank inlet pipeline","Length","21m","RA 39693/05"]
["9.3.4.12","90 OD Class 12 HDPE tank inlet pipeline","Length","31m","RA 39693/06"]
["9.3.4.13","110 NB 90° bend HDPE","Item",24,"SS 4.2.5"]
["9.3.4.14","90 NB 90°  bend HDPE","Item",64,"SS 4.2.5"]
["9.3.4.15","110 NB 45° adjustable elbow","Item",15,"SS 4.2.5"]
["9.3.4.16","90 NB 45° adjustable elbow","Item",15,"SS 4.2.5"]
["9.3.4.17","25 OD Class 12 HDPE drain pipe","Length","1m","SS 4.2.5"]
["9.3.4.18","Gaskets NB 90","Item",12,"SS 4.2.5"]
["9.3.4.19","Gaskets NB 110","Item",53,"RA 39693"]
["9.3.4.20"," 110 NB HDPE adapter complete with stainless steel backing ring","Item",60,"SS 4.2.5"]
["9.3.4.21","90 NB HDPE adapter complete with stainless steel backing ring","Item",60,"SS 4.2.5"]
["9.3.4.22","Water supply line complete with isolation valve  and accessories for washing the roof area connected at the available point as per design.","Set",1,"SS 4.2.5"]
["9.3.4.23","Stubs for 25 OD manual ball valve","Item",12]
["9.3.4.24"]
["9.3.4.25","Existing Drain manual ball valve for the tanks","Item",6]
["9.3.4.26","Exisiting Tank outlet ball valves","Item",6]
["9.3.4.27","Existing Actuated ball valve","Item",6]
["9.3.4.28","Existing Isolation ball valve","Item",12]
["9.3.4.29","Existing Drain manual ball valve for the tank outlet line","Item",6]
["9.3.4.30","Existing Strainer inlet and outlet manual ball valves","Item",8]
["9.3.4.31","Existing Flow totalizer","Item",2]
["9.3.4.32","Existing Manual isolation valve","Item",4]
["9.3.4.33","Existing Manual isolation valves","Item",16]
["9.3.4.34","Exisitng Magnetic level gauges","Item",6]
[]
[]
[]
["9.3.5","Outside The Building/Poly Plant"]
["9.3.5.1","Top sump valve  (DN 150 CS)","Item",1,"SS 4.2.4"]
["9.3.5.2","Sump valve pipe line 150 OD HDPE","Length","3m"]
["9.3.5.3"," DN 15 Polyproplene with Teflon seating air relief valves for the strainers. ","Item",2]
["9.3.5.4","Carriage water valves to water manifold (DN100 CS)","Items",2,"SS 4.2.4"]
["9.3.5.5"," Ball manual valve that feed the Polyelectolyte suction manifold (100 OD CS ball valve)","Item",1,"SS 4.2.4"]
["9.3.5.6","Sump  non contact Ultrasonic level gauge","item",1,"SS 4.3.7        SS 4.4.4",null," "]
[]
["9.3.6","Dosing Lines"]
["9.3.6.1","Labeling for  all the dosing lines to show their destination and pump (either stand-by or duty, e.g. Duty - System A, or Stand-by System A)","SUM",1]
["9.3.6.2","Ensure that all the pipes are colour coded to Rand Water specifications at regular intervals to be advised (e.g. every 5m)","SUM",1]
[]
["9.3.7","Outside Area(Miscellaneous)"]
["9.3.7.1","All bolts and nuts must be consistent, and place all missing bolts, nuts or washers.","SUM",1]
["9.3.7.2","Camlock fitting","Item",6]
["9.3.7.3","Unequal Tee fitting","SUM",1,"SS 4.2.5"]
["9.3.7.4"," U bolts for 75OD pipe","Item",500]
["9.3.7.5","\n140 IPE (2200mm high)","Item",4]
["9.3.7.6","(200 x 200 x 8 ) baseplate","Item",4]
["9.3.7.7"," M14 RAWL BOLTS\n","Item",20]
["9.3.7.8","Pipe clamps for 90 OD HDPE pipe\n","Item",28]
["9.3.7.9","CAT-AND-Mouse level gauge on all tanks","Item",6,"4.2.1"]
[]
["9.3.8","Additional installation items"]
["9.3.8.1","Repositioning of existing HDPE pipe work on the pipe rack to suit the new duty/standby configuration in the pump room (including support)","SUM",1,"SS 4.2.5"]
["Section 9 :  Carried Forward to Summary"]

{"sheet":"10. Electrical","index":9,"n_rows":101,"n_cols":7,"rows_kept":101,"merged":[[3,0,3,6],[7,1,7,6],[15,1,15,6],[22,0,22,2],[24,0,24,5],[25,1,25,6],[48,0,48,2],[50,0,50,5],[60,1,60,6],[71,0,71,2],[73,0,73,5],[99,0,99,4],[99,9,99,11],[100,0,100,6]],"flags":["formulas_cached_only"]}
[null,"Zuikerbosch Pumping Station: ",{"$nulls":4},"Section 10: Electrical"]
[null,"Polyelectrolyte Dosing Plant 2 @ WA1"]
[]
["SECTION 10:  ASSESSMENT, VALIDATION, SUPPLY, DELIVERY AND INSTALLATION OF EQUIPMENT AND MATERIALS"]
["ITEM NUMBER","DESCRIPTION","UNIT","QUANTITY","SYSTEM SPEC. CLAUSE","RATE","AMOUNT"]
[null,"Please refer to the Electrical Engineering specification details and Drawings in order to price for below items. The Contractor’s responsibilities under this project include, but are not limited to, the following items:"]
[]
[null,"10.1 VERIFICATION AND VALIDATION OF THE EXISTING INSTALLATION."]
["10.1.1","400V SWITCHGEAR (The contractor shall confirm 400V Switchgear’s equipment ratings, trace cables, check for labeling, e.t.c)",1,"Sum","SS 4.2.2"]
["10.1.2","SMALL POWER AND LIGHTING (Measure lux levels, test occupancy sensors, trace all circuits, confirm raw & emergency power SP&L is catered for, e.c.t)",1,"Sum","SS 4.4.3"]
["10.1.3","POWER CABLING (Assess cable ratings, trace and develop cable schedule)",1,"Sum","SS 4.4.5"]
["10.1.4","FIRE DETECTION (Assess schematics, test operation and alarms, check connectivity to the security common services)",1,"Sum","SS 4.4.9"]
["10.1.5","CABLE SUPPORT SYSTEMS (Assess cable glanding, cable racks and ladders, cable trenches, cable sleeves and cable entry sealing systems)",1,"Sum","SS 4.4.8      SS4.4.7       SS4.4.6"]
["10.1.6","UNITERRUPTERBLE POWER SUPPLY SYSTEM (Assess UPS supplies, ratings, termination and UPS unit location)",1,"Sum","SS 4.4.10"]
["10.1.7","LIGHTNING PROTECTION AND EARTHING (Conduct soil resistivity tests, assess plant earthing and bonding circuit)",1,"Sum","SS 4.4.11"]
[null,"10.2 DESIGN"]
["10.2.1","SMALL POWER AND LIGHTING (Top bund walkway and access staircase lighting). ",1,"Sum"]
["10.2.2","SUMP PUMP SYSTEM (Including but not limited to; supply and control cabling, control panel, sump level switch) (400V, 4kW Sump Pump provided) ",1,"Sum"]
["10.2.3","CORRECTIVE MEASURES PLAN (Including but not limited to; snag list developed for all the assessments, proposed solutions report and implementation plan.)",1,"Sum"]
[]
[]
[]
["Total Carried Forward "]
["ITEM NUMBER","DESCRIPTION","UNIT","QUANTITY","SYSTEM SPEC. CLAUSE","RATE","AMOUNT"]
["Total  brought Forward  "]
[null,"10.3 SUPPLY"]
["10.3.1","Sump Pump control panel (Including but not limited to the control panel, level switch, protection devices and all accessories required to the complete operation of the sump pump.)",1,"Sum"]
["10.3.2","2.4m high round suitably sized, straight lighting steel pole. Manufactured to fit existing top bund light fittings. (Including but not limited to base and top mounting brackets and all other required accessories.)",6,"Each"]
["10.3.3","Steel walkway SP&L (lights, fittings, cabling and protection devices from point of supply)",1,"Sum"]
["10.3.4","600/1000V PVCSWAPVC INSULATED COPPER CABLE To SANS 1507"]
["10.3.4.1","2.5 mm2, 4 core",50,"m "]
["10.3.4.2","1,5 mm2, 3 core",50,"m "]
["10.3.5","600/1000V PVCSWAPVC INSULATED COPPER CABLE TERMINATIONS TO SANS 1507"]
["10.3.5.1","2,5 mm2, 4 core",2,"No"]
["10.3.5.2","1,5 mm2, 19 core",10,"No"]
["10.3.6","CABLE ENTRY MODULAR SYSTEM ENGINE ROOM CONCRETE WALL."]
["10.3.6.1","Acid proof stainless steel frames (100x100mm)",2,"Sum"]
["10.3.6.2","Modules and round seals to fit through and seal the LV incomer cable. ",1,"Sum"]
["10.3.7","HOT DIPPED GALVANISED, HEAVY DUTY, O-LINE HEAVY DUTY OR EQUIVALENT CABLE RACKING."]
["10.3.7.1","150 mm wide straight run",100,"m"]
["10.3.7.2","150 mm wide tee unit",4,"Unit"]
["10.3.7.3","Cable Rack Accessories and supports",1,"Sum"]
["10.3.8","SUPPLY OF ITEMS RESULTING FROM ASSESMENTS"]
["10.3.8.1","400V SWITCHGEAR (The contractor shall confirm 400V Switchgear’s equipment ratings, trace cables, check for labeling, e.t.c)",1,"Sum"]
["10.3.8.2","SMALL POWER AND LIGHTING (Measure lux levels, test occupancy sensors, trace all circuits, confirm raw & emergency power SP&L is catered for, e.c.t)",1,"Sum"]
["10.3.8.3","POWER CABLING (Assess cable ratings, trace and develop cable schedule)",1,"Sum"]
["10.3.8.4","FIRE DETECTION (Assess schematics, test operation and alarms, check connectivity to the security common services)",1,"Sum"]
[]
["Total Carried Forward "]
["ITEM NUMBER","DESCRIPTION","UNIT","QUANTITY","SYSTEM SPEC. CLAUSE","RATE","AMOUNT"]
["Total  brought Forward  "]
["10.3.8.5","CABLE SUPPORT SYSTEMS (Assess cable glanding, cable racks and ladders, cable trenches, cable sleeves and cable entry sealing systems)",1,"Sum"]
["10.3.8.6","UNITERRUPTERBLE POWER SUPPLY SYSTEM (Assess UPS supplies, ratings, termination and UPS unit location)",1,"Sum"]
["10.3.8.7","LIGHTNING PROTECTION AND EARTHING (Conduct soil resistivity tests, assess plant earthing and bonding circuit)",1,"Sum"]
["10.3.9","Decommission existing round straight lighting steel poles in the top bund area. ",6,"Each"]
["10.3.10","2.4m high round suitably sized, straight lighting steel pole. Manufactured to fit existing top bund light fittings. (Including but not limited to existing lights and fittings, base and top mounting brackets and all other required accessories.)",6,"Each"]
["10.3.11","Steel walkway SP&L (lights, fittings, cabling and protection devices from point of supply) ",1,"Sum"]
["10.3.12","Removal and reinstallation of the pump room lighting, cabling and any other accessories during pipe and pumps rearrangements. ",1,"Sum"]
["10.3.13","Decommissioning of dosing pumps and any other accessories during pipe and pumps rearrangements.",1,"Sum"]
["10.3.14","Reinstalling of dosing pumps and any other accessories during pipe and pumps rearrangements.",1,"Sum"]
[null,"10.4 INSTALL"]
["10.4.1","Sump Pump control panel (Including but not limited to the control panel, level switch, protection devices and all accessories required to the complete operation of the sump pump.)",1,"Sum"]
["10.4.2","2.4m high round suitably sized, straight lighting steel pole. Manufactured to fit existing top bund light fittings. (Including but not limited to base and top mounting brackets and all other required accessories.)",6,"Each"]
["10.4.3","Steel walkway SP&L (lights, fittings, cabling and protection devices from point of supply)",1,"Sum"]
["10.4.4","600/1000V PVCSWAPVC INSULATED COPPER CABLE To SANS 1507"]
["10.4.4.1","2.5 mm2, 4 core",50,"m "]
["10.4.4.2","1,5 mm2, 3 core",100,"m "]
["10.4.5","600/1000V PVCSWAPVC INSULATED COPPER CABLE TERMINATIONS TO SANS 1507"]
["10.4.5.1","2,5 mm2, 4 core",2,"No"]
["10.4.5.2","1,5 mm2, 19 core",20,"No"]
[]
["Total Carried Forward "]
["ITEM NUMBER","DESCRIPTION","UNIT","QUANTITY","SYSTEM SPEC. CLAUSE","RATE","AMOUNT"]
["Total  brought Forward  "]
["10.4.6","CABLE ENTRY MODULAR SYSTEM ENGINE ROOM CONCRETE WALL."]
["10.4.6.1","Acid proof stainless steel frames (100x100mm)",2,"Sum"]
[null,"Modules and round seals to fit through and seal the LV incomer cable. ",null,"Sum"]
["10.4.6.2","Modules and round seals to fit through and seal the LV incomer cable. ",1,"Sum"]
["10.4.7","HOT DIPPED GALVANISED, HEAVY DUTY, O-LINE HEAVY DUTY OR EQUIVALENT CABLE RACKING."]
["10.4.7.1","150 mm wide straight run",100,"m"]
["10.4.7.2","150 mm wide tee unit",4,"Unit"]
["10.4.7.3","Cable Rack Accessories and supports",1,"Sum"]
["10.4.8","INSTALLATION OF ITEMS RESULTING FROM ASSESMENTS"]
["10.4.8.1","400V SWITCHGEAR (The contractor shall confirm 400V Switchgear’s equipment ratings, trace cables, check for labeling, e.t.c)",1,"Sum"]
["10.4.8.2","SMALL POWER AND LIGHTING (Measure lux levels, test occupancy sensors, trace all circuits, confirm raw & emergency power SP&L is catered for, e.c.t)",1,"Sum"]
["10.4.8.3","POWER CABLING (Assess cable ratings, trace and develop cable schedule)",1,"Sum"]
["10.4.8.4","FIRE DETECTION (Assess schematics, test operation and alarms, check connectivity to the security common services)",1,"Sum"]
["10.4.8.5","CABLE SUPPORT SYSTEMS (Assess cable glanding, cable racks and ladders, cable trenches, cable sleeves and cable entry sealing systems)",1,"Sum"]
["10.4.8.6","UNITERRUPTERBLE POWER SUPPLY SYSTEM (Assess UPS supplies, ratings, termination and UPS unit location)",1,"Sum"]
["10.4.8.7","LIGHTNING PROTECTION AND EARTHING (Conduct soil resistivity tests, assess plant earthing and bonding circuit)",1,"Sum"]
["10.4.9","Decommission existing round straight lighting steel poles in the top bund area. ",6,"Each"]
["10.4.10","2.4m high round suitably sized, straight lighting steel pole. Manufactured to fit existing top bund light fittings. (Including but not limited to existing lights and fittings, base and top mounting brackets and all other required accessories.)",6,"Each"]
["10.4.11","Steel walkway SP&L (lights, fittings, cabling and protection devices from point of supply) ",1,"Sum"]
["10.4.12","Removal and reinstallation of the pump room lighting, cabling and any other accessories during pipe and pumps rearrangements. ",1,"Sum"]
["10.4.13","Decommissioning of dosing pumps and any other accessories during pipe and pumps rearrangements.",1,"Sum"]
["10.4.14","Reinstalling of dosing pumps and any other accessories during pipe and pumps rearrangements.",1,"Sum"]
[]
[null,"10.5 SPARES "]
["10.5.1","A maintenance kit shall be offered for each major item of proprietary equipment",1,"Sum"]
["Section 11 :  Carried Forward to Summary"]
["Note: Please refer to the drawings for any line item that might have been missed in the above bill and inform the Project Manager of such items that have been omitted from this bill. For any clarity also refer questions to the same said person."]

{"sheet":"11. Automation","index":10,"n_rows":44,"n_cols":10,"rows_kept":44,"merged":[[3,0,3,11],[4,0,4,11],[5,0,6,0],[5,1,6,1],[5,2,6,2],[5,3,6,3],[5,6,6,6],[5,7,6,8],[5,9,6,11],[7,0,7,11],[8,0,8,11],[9,7,9,8],[9,9,9,11],[10,7,10,8],[10,9,10,11],[11,7,11,8],[11,9,11,11],[12,7,12,8],[12,9,12,11],[13,7,13,8],[13,9,13,11],[14,7,14,8],[14,9,14,11],[15,7,15,8],[15,9,15,11],[16,7,16,8],[16,9,16,11],[17,7,17,8],[17,9,17,11],[18,7,18,8],[18,9,18,11],[19,7,19,8],[19,9,19,11],[20,7,20,8],[20,9,20,11],[22,0,22,2],[23,0,24,0],[23,1,24,1],[23,2,24,2],[23,3,24,3],[23,6,24,6],[23,7,24,8],[23,9,24,11],[25,0,25,5],[26,7,26,8],[26,9,26,11],[27,7,27,8],[27,9,27,11],[28,7,28,8],[28,9,28,11],[29,0,29,11],[30,7,30,8],[30,9,30,11],[31,7,31,8],[31,9,31,11],[32,7,32,8],[32,9,32,11],[33,7,33,8],[33,9,33,11],[34,7,34,8],[34,9,34,11],[35,7,35,8],[35,9,35,11],[36,0,36,11],[37,7,37,8],[37,9,37,11],[38,7,38,8],[38,9,38,11],[40,0,40,11],[41,7,41,8],[41,9,41,11],[42,7,42,8],[42,9,42,11],[43,0,43,8],[43,9,43,11]],"flags":["formulas_cached_only"]}
[null,"Zuikerbosch Pumping Station: ",{"$nulls":4},"Section 11: Automation"]
[null,"Polyelectrolyte Dosing Plant 2 @ WA1"]
[]
["SECTION 11:  SUPPLY, DELIVERY AND INSTALLATION OF EQUIPMENT AND MATERIALS (Refer to Automation  System Specification)"]
["Zuikerbosch Pumping Station – Polyelectrolyte 1 &2"]
["Item No.","Description","System     Spec Clause","Make","Model","Qty","U O M","Rate (B)",null,"Total A*B"]
[{"$nulls":4},"Number","(A)"]
["MCC Room – Automation Equipment’s "]
["11.1. MCC Room – Automation Equipment’s "]
["11..11","supply, install, test and commission of Modbus RTU cable.","System     Spec Clause",null,null,20,"meters"]
["11.1.2","trace, wiring and labelling of two Modbus cables between the magnetic flow meter sensor and the transmitters.","3.1.2.1",null,null,"Sum","Complete"]
["11.1.3","configure, calibrate, test and commission two (2) existing Siemen’s Sitrans FM Mag 6000 magnetic flow meters","3.1.2.2",null,null,"Sum","Complete"]
["11.1.4","supply, install test and commission fluorescent lights inside the PLC panel together with door limit switches","3.1.3.1",null,null,4,"Each"]
["11.1.5","re-route, wire, test and commission eight (8) existing dosing pump I/O cabling wiring between the RIO panels and the dosing pump to match the new duty/standby arrangement","3.2.1.1",null,null,8,"Each"]
["11.1.6","supply, install, test and commission of IScrOAScr I/O signal cable wiring as per the provided cable schedule between the dosing pump and RIO control panel in case the existing cabling does not cater for all pumps.","3.2.1.2",null,null,30,"Meters"]
["11.1.7","re-route, wire, test and commission eight (8) existing actuators I/O cabling wiring between the RIO panels and the actuator to match the new duty/standby arrangement.","3.2.1.3",null,null,8,"Each"]
["11.1.8","supply, install, test and commission of IScrOAScr I/O signal cable wiring as per the provided cable schedule between the dosing pump and RIO control panel in case the existing cabling does not cater for all actuators..","3.2.1.4",null,null,30,"Meters"]
["11.1.9","re-route, wire, test and commission eight (8) existing pressure indication transmitter I/O cabling wiring between the RIO panels and the pressure indication transmitter to match the new duty/standby arrangement","3.2.1.5",null,null,8,"Each"]
["11.1.10","supply, install, test and commission of IScrOAScr signal cable wiring as per the provided cable schedule for discrete I/O between the pressure indication transmitter and RIO control panel in case the existing cabling does not cater for all pressure transmitter.","3.2.1.5",null,null,30,"Meters"]
["11.1.11","re-route, wire, test and commission sixteen (16) {eight carriage water FIT’s and eight polyelectrolyte FIT’s} existing flow indication transmitter IScrOAScr I/O cabling wiring between the RIO panels and the flow indication transmitter to match the new duty/standby arrangement.","3.2.1.6",null,null,16,"Each"]
["11.1.12","supply, install, test and commission thirty (30) meters of screen signal cable wiring as per the provided cable schedule for discrete I/O between the flow indication transmitter and RIO control panel in case the existing cabling does not cater for all flow meters.","3.2.1.7",null,null,30,"Meters"]
[]
["Total Carried Forward "]
["Item No.","Description","System     Spec Clause","Make","Model","Qty","U O M","Rate (B)",null,"Total A*B"]
[{"$nulls":4},"Number","(A)"]
["Total  brought Forward  "]
["11.1.13","configure, calibrate, test and commission thirty-two (32) existing Siemens Sitrans FM MAG 600 magnetic flow meters.","3.2.1.8",null,null,"Sum","Complete"]
["11.1.14","mark and label all automation instrumentation, cabling and equipment that appear on the P&ID and cable schedule","3.2.3.1",null,null,"Sum","Complete"]
["11.1.15","The Contractor shall supply calibration and verification equipment system for the existing Sitrans MAG 500 and 600 flow meters.","3.2.3.2",null,null,"Sum","Complete"]
["11.2 Foyer Area – Automation Equipment’s "]
["11.2.1","supply, Install, test and commission HMI with 4 gig compact flash card in the Poly plant","3.3.1.1",null,null,1,"Each"]
["11.2.2","wire, test and commission one (1) fan according to HMI panel general arrangement RA 29056","3.3.1.2",null,null,1,"Each"]
["11.2.3","design, supply, deliver, install, test and commission biometric fingerprint reader access control system on the main access door of the Polyelectrolyte building which supports Modbus TCP/IP communication protocol.","3.3.2.1",null,null,"Sum","Complete"]
["11.2.4","design, supply, deliver, install, configure, test and commission the signal from the biometric sensor (that will be used for regulating the access into the plant) into a central server system for risk services; the server shall log and show the names of the person who entered the building.","3.3.2.2",null,null,"Sum","Complete"]
["11.2.5","design, supply, deliver, install, configure, test and commission monitoring system for the existing fire detection.","3.3.3.1",null,null,"Sum","Complete"]
["11.2.6","supply, install, test and commission all necessary software’s required for the monitoring of the fire alarm system.","3.3.3.2",null,null,"Sum","Complete"]
["11.3 Top Bund – Automation Equipment’s "]
["11.3.1","re-route, wiring, calibrate, configure, test and commission six (6) existing Siemens Sitrans Probe LU ultrasonic level transmitter to match the new tank layout arrangement and submit calibration reports/certificate to Rand Water.","3.4.1.1",null,null,6,"Each"]
["11.3.2","supply, deliver, replace, install, test, and commission ultrasonic level transmitter as shown on the network layout drawing RA 17929.","3.4.1.2",null,null,3,"each"]
[24,"The Contractor shall supply, install, test and commission all necessary software’s required for the monitoring of the fire alarm system","3.4.3.2",null,null,"Sum","Complete"]
["11.4 Bottom Bund – Automation Equipment’s "]
["11.4.1","supply, deliver, install, calibrate, test, and commission one (1) ultrasonic level sensors in the overflow bund.","3.5.1.1",null,null,1,"Each"]
["11.4.2","supply, deliver, install, test, and commission 30 meters of twisted pair and SWAIScrOAScr multicore I/O cabling between the level instrument and the common service PLC located inside the MCC room","3.5.1.2",null,null,30,"meters"]
["Section 11 :  Carried Forward to Summary"]

{"sheet":"12.Summary","index":11,"n_rows":57,"n_cols":7,"rows_kept":57,"merged":[[30,0,30,1],[33,0,33,1],[34,0,34,1],[35,0,35,1],[38,0,38,1],[41,0,41,1],[44,0,44,1],[47,0,47,1],[48,0,48,1],[49,0,49,1],[52,0,52,1],[54,0,54,2],[56,0,56,2]],"flags":["formulas_cached_only"]}
[null,"Zuikerbosch Pumping Station: ",{"$nulls":4},"Section 11: Automation"]
[null,"Polyelectrolyte Dosing Plant 2 @ WA1"]
[]
["Section","Description                                 SUMMARY  ","AMOUNT"]
[]
[1,"PRELIMINARY AND GENERAL","R                       -"]
[]
[2,"QUALITY CONTROL & ASSURANCE","R                       -"]
[]
[3,"HEALTH AND SAFETY","R                       -"]
[]
[4,"ENVIRONMENTAL","R                       -"]
[]
[5,"CIVIL - SITE CLEARANCE","R                       -"]
[]
[6,"CIVIL - CONCRETE","R                       -"]
[]
[7,"CIVIL - STRUCTURAL STEEL","R                       -"]
[]
[8,"CIVIL - STRUCTURAL STEEL (CORROSION PROTECTION)","R                       -"]
[]
[9,"MECHANICAL","R                       -"]
[]
[10,"ELECTRICAL","R                       -"]
[]
[11,"AUTOMATION","R                       -"]
[]
[]
[]
[]
["SUBTOTAL A ……………………………………..……………………………………………",null,"R                       -"]
[]
[]
["CONTINGENCIES"]
["Add 10% of SUBTOTAL A …………..…………………...…...…………………………….",null,"R                       -"]
["(The Provisional Sum provided here may only be expended at the sole discretion of the Engineer, and the Employer reserves the right, during the execution of the works, to adjust the stated sum downwards or to omit it entirely without affecting the validity of the contract.)"]
[]
[]
["SUBTOTAL B ……..…………..………………………..………….…………………………",null,"R                       -"]
[]
[]
["CONTRACT PRICE ADJUSTMENT (Provisional Allowance)………………………….."]
[]
[]
["SUBTOTAL C ……………………...…..……………………………….……………………."]
[]
[]
["VALUE ADDED TAX"]
["Add 15% of Subtotal C ………..…….……………………..………...……..………………"]
["(Provisional sum based on current rate of VAT)"]
[]
[]
["TOTAL CARRIED TO FORM C1.1, FORM OF OFFER"]
[]
[]
[]
["SIGNED ON BEHALF OF TENDERER: ……………………………………………..……………………………………………."]