{"text_format":"3","workbook":"xls","n_sheets":13,"sheets":["INSTRUCTIONS","Field Equipment","Flow Measurements","Level Measurements","Limit switches","Pressure Measurements","Temperature Measurements","Junction Boxes","Pyrometers","Flame Scanners","Manifolds","Electrical - Control","Electrical - Binary"],"not_rendered":{"images":1,"external_links":1,"defined_names":16},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"INSTRUCTIONS","index":0,"n_rows":6,"n_cols":2,"rows_kept":6,"merged":[[3,1,4,13],[5,1,26,13]],"flags":["formulas_cached_only"]}
[]
[]
[]
[null,"MAJUBA\nAppendix E: \nField Equipment – Technical Schedule"]
[]
[null,"\n\n\n\n\nOver and above the general instructions provided in Section 2 for the Technical Tender Returnables of the Works Information, the following instructions apply to all the Tender Returnables in Appendix H:\n\n1. The information provided by the Tenderer shall be evaluated against the Employer's Works Information 10.4.\n\n2. The Tenderer must complete and submit sheets \"Field Equipment\", “Flow Measurements”, \"Level Measurements\", \"Limits switches\", \"Pressure Measurements\", \" Temperature Measurements\", \"Junction boxes\", \"Manifolds\", \"Electric-Control\", Electric-Binary\", \"Pyrometer\", \"Flame scanner\"  of Appendix E \n\n\n"]

{"sheet":"Field Equipment","index":1,"n_rows":16,"n_cols":12,"rows_kept":16,"merged":[[0,0,0,8],[0,9,0,10],[1,0,1,11],[2,0,2,11],[3,0,3,11],[4,0,4,11],[5,0,5,11],[6,1,6,3],[6,4,6,9],[7,1,7,3],[7,4,7,9],[8,1,8,3],[8,4,8,9],[9,1,9,3],[9,4,9,9],[10,1,10,3],[10,4,10,9],[11,1,11,3],[11,4,11,9],[12,1,12,3],[12,4,12,9],[13,1,13,3],[13,4,13,9],[14,1,14,3],[14,4,14,9],[15,1,15,3],[15,4,15,9]],"flags":["formulas_cached_only"]}
["Field Equipment",{"$nulls":8},"Section:",null,"11.4"]
["All Cells in white must be completed by the Tenderer. Failure to comply with the schedule will be regarded as non-compliance. Cells in cream may be optionally completed by the Tenderer as required"]
[]
["A. Product Information"]
["11.4 FIELD EQUIPMENT"]
[]
["No.","Enquiry Information Required",null,null,"Tenderer's response",{"$nulls":5},"Datsheet/ Reference","Tenderer's additional information"]
["a","Confirmation that all field equipment & installations shall comply with 240-56355754 - Field Instrument Installation Standard."]
["b","Confirmation that all field equipment & installations shall comply with 240-56355815 - Junction Boxes and Cable Termination Standard."]
["c","Confirmation that all field equipment & installations shall comply withiii. 240-56355843 - Pressure Measurement Systems Installation Standard."]
["d","Confirmation that all field equipment & installations shall comply with iv. 240-56355888 - Temperature Measurement Systems Installation Standard."]
["e","Confirmation that all field equipment shall operate over an ambient temperature range of: -10C to 70C"]
["f","Confirmation that all field equipment offered are suitable for use in the zone in which it is installed as perper SANS 10108 (6th edition 2017)  "]
["g","Confirmation that all field equipment excluding junction/splitter boxes and their electrical connections shall be rated IP 67."]
["h","Confirmation that Junction/splitter boxes and their electrical connections shall be rated IP 65."]
["i","Confirmation that all analogue field equipment shall be HART devices."]

{"sheet":"Flow Measurements","index":2,"n_rows":25,"n_cols":9,"rows_kept":25,"merged":[[2,1,3,3],[2,5,3,5],[2,6,3,6],[2,7,3,7],[2,8,3,8],[4,2,5,3]],"flags":["formulas_cached_only"]}
[null,"POWER STATION"]
[null,"INSTRUMENTATION TECHNICAL INFORMATION"]
[null," FLOW MEASUREMENT"]
[]
[null,1,"TRANSMITTERS",null,null,"MAGNETIC","VORTEX","TURBINE","DIFFERENTIAL"]
[{"$nulls":8},"PRESSURE"]
[null,null,1.1,"TRANSMITTER MODEL NUMBER"]
[]
[null,null,"1.2","IP RATING"]
[]
[null,null,1.3,"FULL SCALE ACCURACY"]
[]
[null,null,1.4,"LONG TERM STABILITY"]
[]
[null,null,"1.5","SHORT TERM STABILITY"]
[{"$nulls":3}," (REPEATABILITY)"]
[null,null,1.6,"RESPONSE TIME"]
[]
[null,null,1.7,"POWER REQUIREMENTS"]
[]
[null,null,"1.8","EMC STANDARDS"]
[]
[null,null,1.9,"HART"]
[]
[null,null,"1.10","GUARANTEES DURATION"]

{"sheet":"Level Measurements","index":3,"n_rows":27,"n_cols":11,"rows_kept":27,"merged":[[2,1,3,3],[2,5,3,5],[2,6,3,6],[2,7,3,7],[2,8,3,8],[2,9,3,9],[2,10,3,10],[4,2,5,3]],"flags":["formulas_cached_only"]}
[null,"POWER STATION "]
[null,"INSTRUMENTATION TECHNICAL INFORMATION"]
[null,"LEVEL MEASUREMENT"]
[]
[null,1,"TRANSMITTERS",null,null,"DIFFERENTIAL","ULTRASONIC","RADAR","CAPACITANCE","HYDROSTATIC","GUIDED WAVE "]
[{"$nulls":5},"PRESSURE",{"$nulls":4},"RADAR"]
[null,null,1.1,"TRANSMITTER MODEL NUMBER"]
[]
[null,null,"1.2","IP RATING"]
[]
[null,null,1.3,"FULL SCALE ACCURACY"]
[]
[null,null,1.4,"LONG TERM STABILITY"]
[]
[null,null,"1.5","SHORT TERM STABILITY"]
[{"$nulls":3}," (REPEATABILITY)"]
[null,null,1.6,"RESPONSE TIME"]
[]
[null,null,1.7,"POWER REQUIREMENTS"]
[]
[null,null,"1.8","EMC STANDARDS"]
[]
[null,null,1.9,"HART"]
[]
[null,null,"1.10","GUARANTEES DURATION"]
[]
[null,null,1.11,"SIL RATING"]

{"sheet":"Limit switches","index":4,"n_rows":25,"n_cols":4,"rows_kept":25,"merged":[[2,1,3,3],[2,5,3,5],[2,6,3,6],[2,7,3,7],[2,8,3,8],[2,9,3,9],[4,2,5,3]],"flags":["formulas_cached_only"]}
[null,"POWER STATION "]
[null,"INSTRUMENTATION TECHNICAL INFORMATION"]
[null,"LIMITS AND PROXIMITY SWITCHES"]
[]
[null,1,"SWITCHES"]
[]
[null,null,1.1," MODEL NUMBER"]
[]
[null,null,"1.2","IP RATING"]
[]
[null,null,1.3,"WIRE BREAK DETECTION"]
[]
[null,null,1.4,"LONG TERM STABILITY"]
[]
[null,null,"1.5","SHORT TERM STABILITY"]
[{"$nulls":3}," (REPEATABILITY)"]
[null,null,1.6,"RESPONSE TIME"]
[]
[null,null,1.7,"ELECTRICAL RATING"]
[]
[null,null,"1.8","EMC STANDARDS"]
[]
[null,null,1.9,"GUARANTEES DURATION"]
[]
[null,null,"1.10"]

{"sheet":"Pressure Measurements","index":5,"n_rows":27,"n_cols":8,"rows_kept":27,"merged":[[2,1,3,3],[2,5,3,5],[2,6,3,6],[2,7,3,7],[4,2,5,3]],"flags":["formulas_cached_only"]}
[null,"POWER STATION"]
[null,"INSTRUMENTATION TECHNICAL INFORMATION"]
[null,"PRESSURE MEASUREMENT "]
[]
[null,1,"PRESSURE TRANSMITTER ",null,null,"DIFFERENTIAL","PRESSURE","PRESSURE"]
[{"$nulls":5},"PRESSURE",null,"SWITCH"]
[null,null,1.1," MODEL NUMBER"]
[]
[null,null,"1.2","IP RATING"]
[]
[null,null,1.3,"ACCURACY"]
[]
[null,null,1.4,"LONG TERM STABILITY"]
[]
[null,null,"1.5","SHORT TERM STABILITY"]
[{"$nulls":3}," (REPEATABILITY)"]
[null,null,1.6,"RESPONSE TIME"]
[]
[null,null,1.7,"POWER REQUIREMENTS"]
[]
[null,null,"1.8","EMC STANDARDS"]
[]
[null,null,1.9,"HART"]
[]
[null,null,"1.10","GUARANTEES DURATION"]
[]
[null,null,1.11,"SIL RATING"]

{"sheet":"Temperature Measurements","index":6,"n_rows":27,"n_cols":7,"rows_kept":27,"merged":[[2,1,3,3],[2,5,3,5],[2,6,3,6],[2,7,3,7],[2,8,3,8],[2,9,3,9],[2,10,3,10],[2,11,3,11],[2,12,3,12],[2,13,3,13],[2,14,3,14],[2,15,3,15],[2,16,3,16],[4,2,5,3]],"flags":["formulas_cached_only"]}
[null,"POWER STATION "]
[null,"INSTRUMENTATION TECHNICAL INFORMATION"]
[null,"TEMPERATURE MEASUREMENT "]
[]
[null,1,"TRANSMITTER",null,null,"TYPE J","TYPE K"]
[]
[null,null,1.1," MODEL NUMBER"]
[]
[{"$nulls":3},"CONVERTER MODULE MOUNTING"]
[]
[null,null,"1.2","IP RATING"]
[]
[null,null,1.3,"ACCURACY"]
[]
[null,null,1.4,"LONG TERM STABILITY"]
[]
[null,null,"1.5","SHORT TERM STABILITY"]
[{"$nulls":3}," (REPEATABILITY)"]
[null,null,1.6,"RESPONSE TIME"]
[]
[null,null,1.7,"POWER REQUIREMENTS"]
[]
[null,null,"1.8","EMC STANDARDS"]
[]
[null,null,1.9,"COMPENSATING LEAD TYPE"]
[]
[null,null,"1.10","GUARANTEES DURATION"]

{"sheet":"Junction Boxes","index":7,"n_rows":27,"n_cols":9,"rows_kept":27,"merged":[[4,2,5,4],[4,6,5,6],[4,7,5,7],[4,8,5,8],[6,3,7,4]],"flags":["formulas_cached_only"]}
[]
[]
[null,null,"POWER STATION "]
[null,null,"INSTRUMENTATION TECHNICAL INFORMATION"]
[null,null,"Enclosures"]
[]
[null,null,1,"Junction Boxes and LCP'S",null,null,"JB'S","LCP'S","Splitter Boxes"]
[]
[{"$nulls":3},1.1,"MATERIAL"]
[]
[{"$nulls":3},"1.2","COATING"]
[]
[{"$nulls":3},1.3,"IP RATING"]
[]
[{"$nulls":3},1.4,"CABLE ENTRY"]
[]
[{"$nulls":3},1.5,"START BUTTON"]
[]
[{"$nulls":3},1.6,"STOP BUTTON"]
[]
[{"$nulls":3},1.7,"COLOUR CODING"]
[]
[{"$nulls":3},1.8,"MOUNTING BRACKETS"]
[]
[{"$nulls":3},1.9,"HINGES"]
[]
[{"$nulls":3},1.1," LOCKING"]

{"sheet":"Pyrometers","index":8,"n_rows":29,"n_cols":4,"rows_kept":29,"merged":[[2,1,3,4],[2,5,3,5],[2,6,3,6],[2,7,3,7],[2,8,3,8],[2,9,3,9],[2,10,3,10],[2,11,3,11],[2,12,3,12],[2,13,3,13],[2,14,3,14],[2,15,3,15],[2,16,3,16],[4,2,5,3],[30,2,30,6]],"flags":["formulas_cached_only"]}
[null,"POWER STATION "]
[null,"INSTRUMENTATION TECHNICAL INFORMATION"]
[null,"PYROMETERS"]
[]
[]
[]
[null,null,1.1," MODEL NUMBER"]
[]
[null,null,"1.2","PROGRAMMING INTERFACE"]
[]
[null,null,1.3,"MEASUREMENT RANGE"]
[]
[null,null,1.4,"OPERATING TEMPERATURE RANGE"]
[]
[null,null,"1.5","IP RATING"]
[]
[null,null,1.6,"RESPONSE TIME (FOR MEASURE TEMPS >=1000 Deg C)"]
[]
[null,null,1.7,"SIL RATING"]
[]
[null,null,"1.8","POWER REQUIREMENTS"]
[]
[null,null,1.9,"EMC STANDARDS"]
[]
[null,null,"1.10","COOLING MEDIUM (IF REQUIRED)"]
[]
[null,null,1.11,"OVERHEATING FAILURE MODE"]
[]
[null,null,1.12,"GUARANTEES DURATION"]

{"sheet":"Flame Scanners","index":9,"n_rows":31,"n_cols":4,"rows_kept":31,"merged":[[2,1,3,4],[2,5,3,5],[2,6,3,6],[2,7,3,7],[2,8,3,8],[2,9,3,9],[2,10,3,10],[2,11,3,11],[2,12,3,12],[2,13,3,13],[2,14,3,14],[2,15,3,15],[2,16,3,16],[4,2,5,3],[32,2,32,6]],"flags":["formulas_cached_only"]}
[null,"POWER STATION "]
[null,"INSTRUMENTATION TECHNICAL INFORMATION"]
[null,"Flame Scanners"]
[]
[]
[]
[null,null,1.1," MODEL NUMBER"]
[]
[null,null,"1.2","PROGRAMMING / TUNING  INTERFACE"]
[]
[null,null,1.3,"FlAME SENSOR TYPE (UV/IR/UV&IR)"]
[]
[null,null,1.4,"OPERATING TEMPERATURE RANGE"]
[]
[null,null,"1.5","IP RATING"]
[]
[null,null,1.6,"RESPONSE TIME (FLAME ON<1 sec)"]
[]
[null,null,1.7,"SIL RATING"]
[]
[null,null,"1.8","POWER REQUIREMENTS"]
[]
[null,null,1.9,"EMC STANDARDS"]
[]
[null,null,"1.10","FAILURE POSITION"]
[]
[null,null,1.11,"ON BOARD TUNING WITH DISPLAY (Yes/No)"]
[]
[null,null,1.12,"Electrical Connection type ( Quick disconnect etc..)"]
[]
[null,null,1.13,"GUARANTEES DURATION"]

{"sheet":"Manifolds","index":10,"n_rows":17,"n_cols":6,"rows_kept":17,"merged":[[4,3,5,5],[4,7,5,7],[4,8,5,8],[6,4,7,5]],"flags":["formulas_cached_only"]}
[]
[]
[{"$nulls":3},"POWER STATION "]
[{"$nulls":3},"INSTRUMENTATION TECHNICAL INFORMATION"]
[{"$nulls":3},"Manifolds"]
[]
[]
[]
[{"$nulls":4},1.1,"MATERIAL"]
[]
[{"$nulls":4},"1.2","COATING"]
[]
[{"$nulls":4},1.3,"TRANSITION PIECE"]
[]
[{"$nulls":4},1.4,"MODEL NO"]
[]
[{"$nulls":4},1.5,"SEALING MATERIAL"]

{"sheet":"Electrical - Control","index":11,"n_rows":83,"n_cols":11,"rows_kept":83,"merged":[[2,1,3,4],[2,6,3,6],[2,7,3,7],[2,8,3,8],[2,9,3,9],[2,10,3,10],[4,2,5,4],[29,2,30,4],[37,2,38,4]],"flags":["formulas_cached_only"]}
[null,"DUVHA POWER STATION REFURBISHMENT"]
[null,"ACTUATOR TECHNICAL INFORMATION"]
[null,"380V AC ELECTRICAL INTEGRATED SWITCHGEAR ACTUATED CONTROL DAMPER/VANE/VALVE",{"$nulls":4},"                      <60 Nm"," >60 to <120 Nm"," >120 to <250 Nm   "," >250 to <1000 Nm"," >1000 Nm"]
[]
[null,1,"ACTUATOR"]
[]
[null,null,1.1,"IP RATING"]
[]
[null,null,1.2,"ACTUATOR MODEL NUMBERS"]
[{"$nulls":3},"1.2.1","Multi-turn"]
[]
[{"$nulls":3},"1.2.2","1/4 Turn"]
[]
[{"$nulls":3},"1.2.3","Standard Linear Turn(not modified multi-turn)"]
[]
[{"$nulls":3},"1.2.4","For Linier bases with pivot suspension are included"]
[{"$nulls":4},"For Linear bases with pivot suspension are included"]
[null,null,1.3,"SIZING THE ACTUATOR (Nm)"]
[]
[null,null,1.4,"MOTOR DUTY CYCLE"]
[]
[null,null,1.5,"NOMINAL CURRENT  Amps"]
[]
[null,null,1.6,"NO LOAD CURRENT   Amps"]
[]
[null,null,1.7,"STARTING CURRENT   Amps"]
[]
[null,null,1.8,"POWER FACTOR AT RATED TORQUE  cos€"]
[]
[null,2,"FEED BACK ARRANGEMENT"]
[]
[null,null,2.1,null,"POSITION TRANSMITTER MODEL NUMBERS"]
[]
[null,null,2.2,null,"TORQUE AND LIMIT SWITCHES ARRANGEMENTS"]
[]
[null,null,2.3,null,"CONNECTING PLUG TYPE(Provide technical detail)"]
[]
[null,3,"THYRISTER INTEGRAL SWITCHGEAR "]
[]
[null,null,3.1,null," INTEGRAL SWITCHGEAR MODEL NUMBERS"]
[]
[null,null,3.2,null,"THREE LOCKABLE POSITION INCLUDED (Y/N)(Provide technical detail)"]
[]
[null,null,3.3,null,"DUTY CYCLE"]
[]
[null,null,3.4,null,"NOMINAL CURRENT  Amps"]
[]
[null,null,3.5,null,"NO LOAD CURRENT   Amps"]
[]
[null,null,3.6,null,"STARTING CURRENT   Amps"]
[]
[null,null,3.7,null,"CONNECTING PLUG TYPE(Provide technical detail)"]
[]
[null,4,"LINKAGES AND ADAPTER FLANGES"]
[]
[null,null,4.1,null,"Adapter flanges between actuator & valve are included.(Provide technical detail)."]
[]
[null,null,4.2,null,"Adapter linkages between actuator & damper are included.(Provide technical detail)."]
[]
[null,5,"GEARBOXES "]
[]
[null,null,5.1,null,"GEARBOXES  MODEL NUMBER NUMBERS"]
[]
[null,null,5.2,null,"GEARBOXES RATIO"]
[]
[null,null,5.3,null,"Counterclockwise gearboxes are provided with clockwise actuators (Linear, 1/4 Turn & Multi-turn) (Y/N)"]
[]
[null,null,5.4,null,"Quarter turn gearboxes the worm gear is a 360° gear (Y/N)"]
[]
[null,null,5.5,null,"Bronze worm wheels provided on quarter turn modulating gearboxes (Y/N)"]
[]
[null,null,5.6,null,"Lever arm quarter turn gearboxes form part of a standard product range (Y/N) provide technical details "]
[]
[null,6,"INTEGRAL STARTER/SWITCHGEAR - SPLIT ARRANGEMENT"]
[]
[null,null,6.1,null,"Can the integral starter be split away from actuators offered?"]
[]
[null,null,6.2,null,"If yes, are the brackets custom made or standard off the shelf?"]
[]
[null,null,6.3,null,"Confirm that fly leads are included in the applications requiring starter to be split from the actuator?"]
[]
[null,7,"GUARANTEES"]
[null,null,"GUARANTEES DURATION"]

{"sheet":"Electrical - Binary","index":12,"n_rows":59,"n_cols":11,"rows_kept":59,"merged":[[2,1,3,4],[2,6,3,6],[2,7,3,7],[2,8,3,8],[2,9,3,9],[2,10,3,10],[4,2,5,4],[29,2,30,4]],"flags":["formulas_cached_only"]}
[null,"DUVHA POWER STATION REFURBISHMENT"]
[null,"ACTUATOR TECHNICAL INFORMATION"]
[null,"380V AC ELECTRICAL NON-INTEGRATED SWITCHGEAR ACTUATED BINARY VALVE",{"$nulls":4}," <60 Nm",">60 to <120 Nm"," >120 to <250 Nm   ",">250 to <1000 Nm"," >1000 Nm"]
[]
[null,1,"ACTUATOR"]
[]
[null,null,1.1,"IP RATING"]
[]
[null,null,1.2,"ACTUATOR MODEL NUMBERS"]
[{"$nulls":3},"1.2.1","Multi-turn"]
[]
[{"$nulls":3},"1.2.2","1/4 Turn"]
[]
[{"$nulls":3},"1.2.3","Standard Linear Turn(not modified multi-turn)"]
[]
[{"$nulls":3},"1.2.4","For Linier bases with pivot suspension are included"]
[{"$nulls":4},"For Linear bases with pivot suspension are included"]
[null,null,1.3,"SIZING THE ACTUATOR (Nm)"]
[]
[null,null,1.4,"MOTOR DUTY CYCLE"]
[]
[null,null,1.5,"NOMINAL CURRENT  Amps"]
[]
[null,null,1.6,"NO LOAD CURRENT   Amps"]
[]
[null,null,1.7,"STARTING CURRENT   Amps"]
[]
[null,null,1.8,"POWER FACTOR AT RATED TORQUE  cos€"]
[]
[null,2,"FEED BACK ARRANGEMENT"]
[]
[null,null,2.1,null,"POSITION TRANSMITTER MODEL NUMBERS"]
[]
[null,null,2.2,null,"TORQUE AND LIMIT SWITCHES ARRANGEMENTS"]
[]
[null,null,2.3,null,"CONNECTING PLUG TYPE(Provide technical detail)"]
[]
[null,3,"LINKAGES AND ADAPTER FLANGES"]
[]
[null,null,4.1,null,"Adapter flanges between actuator & valve are included.(Provide technical detail)."]
[]
[null,null,4.2,null,"Adapter linkages between actuator & damper are included.(Provide technical detail)."]
[]
[null,4,"GEARBOXES "]
[]
[null,null,5.1,null,"GEARBOXES  MODEL NUMBER NUMBERS"]
[]
[null,null,5.2,null,"GEARBOXES RATIO"]
[]
[null,null,5.3,null,"Counterclockwise gearboxes are provided with clockwise actuators (Linear, 1/4 Turn & Multi-turn) (Y/N)"]
[]
[null,null,5.4,null,"Quarter turn gearboxes the worm gear is a 360° gear (Y/N)"]
[]
[null,null,5.5,null,"Bronze worm wheels provided on quarter turn modulating gearboxes (Y/N)"]
[]
[null,null,5.6,null,"Lever arm quarter turn gearboxes form part of a standard product range (Y/N) provide technical details "]
[]
[null,7,"GUARANTEES"]
[null,null,"GUARANTEES DURATION"]