{"text_format":"3","workbook":"xlsx","n_sheets":21,"sheets":["Schedule 1","Schedule 2","Schedule 3","Schedule 4","Schedule 5","Schedule 6","Schedule 7","Schedule 8","Schedule 9","Schedule 10","Schedule 11","Schedule 12","Schedule 13","Schedule 14","Schedule 15","Schedule 16","Schedule 17","Schedule 18","Schedule 19","Summary Of Schedules","Rate Estimator"],"not_rendered":{"comments":19},"read":"whole","date_system":"1900"}

{"sheet":"Schedule 1","index":0,"n_rows":342,"n_cols":8,"rows_kept":342}
["Rate=G","SCHEDULE 1 - PRELIMINARY AND GENERAL"]
["<NewDataSet>·  <xs:schema id=\"NewDataSet\" xmlns=\"\" xmlns:xs=\"http://www.w3.org/2001/XMLSchema\" xmlns:msdata=\"urn:schemas-microsoft-com:xml-msdata\">·    <xs:element name=\"NewDataSet\" msdata:IsDataSet=\"true\" msdata:MainDataTable=\"SummaryItems\" msdata:UseCurrentLocale=\"true\">·      <xs:complexType>·        <xs:choice minOccurs=\"0\" maxOccurs=\"unbounded\">·          <xs:element name=\"SummaryItems\">·            <xs:complexType>·              <xs:sequence>·                <xs:element name=\"ContractNo\" type=\"xs:short\" minOccurs=\"0\" />·                <xs:element name=\"ScheduleNo\" type=\"xs:short\" minOccurs=\"0\" />·                <xs:element name=\"SortNo\" type=\"xs:short\" minOccurs=\"0\" />·                <xs:element name=\"Item\" type=\"xs:string\" minOccurs=\"0\" />·                <xs:element name=\"SubTotalText\" type=\"xs:string\" minOccurs=\"0\" />·                <xs:element name=\"Description\" type=\"xs:string\" minOccurs=\"0\" />·                <xs:element name=\"CalcType\" type=\"xs:string\" minOccurs=\"0\" />·                <xs:element name=\"CalcValue\" type=\"xs:double\" minOccurs=\"0\" />·                <xs:element name=\"UseFirstSubTotal\" type=\"xs:boolean\" minOccurs=\"0\" />·                <xs:element name=\"ExclFromWorks\" type=\"xs:boolean\" minOccurs=\"0\" />·                <xs:element name=\"ExclFromProjected\" type=\"xs:boolean\" minOccurs=\"0\" />·              </xs:sequence>·            </xs:complexType>·          </xs:element>·        </xs:choice>·      </xs:complexType>·    </xs:element>·  </xs:schema>·</NewDataSet>",{"$nulls":6},"SECTION 1.1: FIXED CHARGED ITEMS"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[1688,"1.1","SABS 1200 A","PRELIMINARY AND GENERAL FIXED CHARGED ITEMS"]
[]
[2246,"1.1.1","8.3.1","CONTRACTUAL REQUIREMENTS"]
[]
[1690,"1.1.1.1","8.3.1","Contractual Requirements for the duration of the Contract","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E8 = CHAR(37), F8*G8/100,F8*G8)","v":{"v":0,"d":"0.00"}}]
[]
[1691,"1.1.2","8.3.2.1","ESTABLISH FACILITIES ON THE SITE (SABS 1200 AB):"]
[]
[1692,"1.1.2.1","8.3.2.1 (a)\r\nPSAB 3.2","Furnished office building for Engineer & Employer including parking (2 No.)","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E12 = CHAR(37), F12*G12/100,F12*G12)","v":{"v":0,"d":"0.00"}}]
[]
[1693,"1.1.2.2","8.3.2.1 (b)\r\nPSAB 4.1","Airtime and wireless internet facilities for Engineer and Employer","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E14 = CHAR(37), F14*G14/100,F14*G14)","v":{"v":0,"d":"0.00"}}]
[]
[1694,"1.1.2.3","PSAB 3.2","Meeting room facilities.","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E16 = CHAR(37), F16*G16/100,F16*G16)","v":{"v":0,"d":"0.00"}}]
[]
[2079,"1.1.2.4","8.3.2.1 (c) PSAB 3.1","Project name board (2 No.) Refer to C4.3 for details ","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E18 = CHAR(37), F18*G18/100,F18*G18)","v":{"v":0,"d":"0.00"}}]
[]
[2550,"1.1.2.5","PS 3.6.5.3","Ablution facilities for Engineer and Employer","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E20 = CHAR(37), F20*G20/100,F20*G20)","v":{"v":0,"d":"0.00"}}]
[]
[25630,"1.1.2.6","PSAB3.3","Temporary Offices for Employers Personnel","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E22 = CHAR(37), F22*G22/100,F22*G22)","v":{"v":0,"d":"0.00"}}]
[]
[1695,"1.1.3","8.3.2.2","ESTABLISH FACILITIES ON THE SITE FOR CONTRACTOR:"]
[]
[1696,"1.1.3.1","8.3.2.2 (a)","Offices & storage sheds","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E26 = CHAR(37), F26*G26/100,F26*G26)","v":{"v":0,"d":"0.00"}}]
[]
[1697,"1.1.3.2","8.3.2.2 (e)","Ablution & latrine facilities","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E28 = CHAR(37), F28*G28/100,F28*G28)","v":{"v":0,"d":"0.00"}}]
[]
[1698,"1.1.3.3","8.3.2.2 (f)","Tools & equipment","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E30 = CHAR(37), F30*G30/100,F30*G30)","v":{"v":0,"d":"0.00"}}]
[]
[1699,"1.1.3.4","8.3.2.2 (g)\r\nPS 3.6","Water supplies, electric power and communications","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E32 = CHAR(37), F32*G32/100,F32*G32)","v":{"v":0,"d":"0.00"}}]
[]
[1700,"1.1.3.5","8.3.2.2 (h)\r\nPS 4.7\r\nPSA 8.8","Dealing with water","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E34 = CHAR(37), F34*G34/100,F34*G34)","v":{"v":0,"d":"0.00"}}]
[]
[1701,"1.1.3.6","8.3.2.2 (i)","Access","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E36 = CHAR(37), F36*G36/100,F36*G36)","v":{"v":0,"d":"0.00"}}]
[]
[1899,"1.1.3.7","8.3.4","Removal of site establishment","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E38 = CHAR(37), F38*G38/100,F38*G38)","v":{"v":0,"d":"0.00"}}]
[]
[7889,"1.1.3.8","PSA 8.3.5","De-establishment of site (provisional quantity)","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E40 = CHAR(37), F40*G40/100,F40*G40)","v":{"v":0,"d":"0.00"}}]
[]
[10541,"1.1.3.9","PSA 8.3.6","Re-establishment on site (provisional quantity)","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E42 = CHAR(37), F42*G42/100,F42*G42)","v":{"v":0,"d":"0.00"}}]
[]
[9461,"1.1.3.10","PEM, PS4.12","Environmental Management Plan Obligations ","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E44 = CHAR(37), F44*G44/100,F44*G44)","v":{"v":0,"d":"0.00"}}]
[]
[9462,"1.1.3.11","PS 4.13","Site security for the duration of the contract ","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E46 = CHAR(37), F46*G46/100,F46*G46)","v":{"v":0,"d":"0.00"}}]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H4:H47)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 1 - PRELIMINARY AND GENERAL"]
[{"$nulls":7},"SECTION 1.1: FIXED CHARGED ITEMS"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H48","v":{"v":0,"d":"0.00"}}]
[7890,"1.1.4","PSOH, PS4.21","OCCUPATIONAL HEALTH & SAFETY"]
[]
[7891,"1.1.4.1",null,"General safety (Fixed Charges)","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E55 = CHAR(37), F55*G55/100,F55*G55)","v":{"v":0,"d":"0.00"}}]
[]
[7892,"1.1.4.2",null,"Health & safety plan","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E57 = CHAR(37), F57*G57/100,F57*G57)","v":{"v":0,"d":"0.00"}}]
[]
[10680,"1.1.4.3",null,"Contractors responsibility in terms of Quality Assurance, Construction Records and Construction Dossier","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E59 = CHAR(37), F59*G59/100,F59*G59)","v":{"v":0,"d":"0.00"}}]
[]
[1703,"1.1.5",null,"ALLOW FOR THE FOLLOWING ADDITIONAL ITEMS WHICH THE TENDERER REQUIRES TO BE PRICED SEPARATELY"]
[]
[10681,null,null,"Note: A breakdown to be attached for each additional item"]
[]
[1704,"1.1.5.1",null,"a)","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E65 = CHAR(37), F65*G65/100,F65*G65)","v":{"v":0,"d":"0.00"}}]
[]
[1705,"1.1.5.2",null,"b)","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E67 = CHAR(37), F67*G67/100,F67*G67)","v":{"v":0,"d":"0.00"}}]
[]
[1706,"1.1.5.3",null,"c)","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E69 = CHAR(37), F69*G69/100,F69*G69)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":35}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H52:H104)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 1 - PRELIMINARY AND GENERAL"]
[{"$nulls":7},"SECTION 1.2: TIME RELATED ITEMS"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[1957,"1.2","SABS 1200 A","PRELIMINARY AND GENERAL TIME RELATED ITEMS"]
[]
[2069,null,null,"Operation and maintenance of facilities on site, for duration of construction, except where otherwise stated:"]
[]
[2247,"1.2.1",null,"CONTRACTUAL REQUIREMENTS"]
[]
[1977,"1.2.1.1","8.4.1","Contractual Requirements for the duration of the Contract","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E115 = CHAR(37), F115*G115/100,F115*G115)","v":{"v":0,"d":"0.00"}}]
[]
[1978,"1.2.2","8.4.2.1","FACILITIES FOR ENGINEER FOR DURATION OF CONSTRUCTION (SABS 1200 AB):"]
[]
[2072,"1.2.2.1","PSAB 3.2\r\n8.4.2.1(a)","Furnished offices for Engineer and Employer including parking (2 No.)","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E119 = CHAR(37), F119*G119/100,F119*G119)","v":{"v":0,"d":"0.00"}}]
[]
[2073,"1.2.2.2","8.4.2.1(b)\r\nPSAB 4.1","Airtime and wireless internet for Engineer and Employer","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E121 = CHAR(37), F121*G121/100,F121*G121)","v":{"v":0,"d":"0.00"}}]
[]
[2076,"1.2.2.3","PSAB 3.2","Meeting room facilities","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E123 = CHAR(37), F123*G123/100,F123*G123)","v":{"v":0,"d":"0.00"}}]
[]
[2552,"1.2.2.4","PS3.6.5.3","Ablution facilities for Engineer and Employer","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E125 = CHAR(37), F125*G125/100,F125*G125)","v":{"v":0,"d":"0.00"}}]
[]
[25631,"1.2.2.5","PSAB3.3","Temporary Offices for Employers Personnel","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E127 = CHAR(37), F127*G127/100,F127*G127)","v":{"v":0,"d":"0.00"}}]
[]
[1983,"1.2.3","8.4.2.2","FACILITIES FOR CONTRACTOR FOR DURATION OF CONSTRUCTION:"]
[]
[2020,"1.2.3.1","8.4.2.2 (a)","Offices & storage sheds","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E131 = CHAR(37), F131*G131/100,F131*G131)","v":{"v":0,"d":"0.00"}}]
[]
[2023,"1.2.3.2","8.4.2.2 (e)","Ablution & latrine facilities","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E133 = CHAR(37), F133*G133/100,F133*G133)","v":{"v":0,"d":"0.00"}}]
[]
[2024,"1.2.3.3","8.4.2.2 (f)","Tools & equipment","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E135 = CHAR(37), F135*G135/100,F135*G135)","v":{"v":0,"d":"0.00"}}]
[]
[2025,"1.2.3.4","8.4.2.2 (g)\r\nPS3.6","Water supplies, electric power and communications","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E137 = CHAR(37), F137*G137/100,F137*G137)","v":{"v":0,"d":"0.00"}}]
[]
[2026,"1.2.3.5","8.4.2.2 (h)\r\nPSA 8.8","Dealing with water","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E139 = CHAR(37), F139*G139/100,F139*G139)","v":{"v":0,"d":"0.00"}}]
[]
[2027,"1.2.3.6","8.4.2.2 (i)","Access","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E141 = CHAR(37), F141*G141/100,F141*G141)","v":{"v":0,"d":"0.00"}}]
[]
[2029,"1.2.3.7","8.4.3\r\nPS 4\r\nPS 4.14","Supervision for the duration of the Contract","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E143 = CHAR(37), F143*G143/100,F143*G143)","v":{"v":0,"d":"0.00"}}]
[]
[2030,"1.2.3.8","8.4.4","Company and head office overhead costs for the duration of the Contract","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E145 = CHAR(37), F145*G145/100,F145*G145)","v":{"v":0,"d":"0.00"}}]
[]
[9458,"1.2.3.9","PS4.12\r\nPEM","Environmental Management Plan Obligations","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E147 = CHAR(37), F147*G147/100,F147*G147)","v":{"v":0,"d":"0.00"}}]
[]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H109:H149)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 1 - PRELIMINARY AND GENERAL"]
[{"$nulls":7},"SECTION 1.2: TIME RELATED ITEMS"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H150","v":{"v":0,"d":"0.00"}}]
[9459,"1.2.3.10","PS4.13","Site security for the duration of the contract","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E155 = CHAR(37), F155*G155/100,F155*G155)","v":{"v":0,"d":"0.00"}}]
[]
[10540,"1.2.3.11",null,"Communication and Public Relations","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E157 = CHAR(37), F157*G157/100,F157*G157)","v":{"v":0,"d":"0.00"}}]
[]
[7897,null,"8.4.5","Other time-related obligations (Contractor to Specify)  "]
[]
[7898,"1.2.3.12",null,"a)","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E161 = CHAR(37), F161*G161/100,F161*G161)","v":{"v":0,"d":"0.00"}}]
[]
[7899,"1.2.3.13",null,"b)","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E163 = CHAR(37), F163*G163/100,F163*G163)","v":{"v":0,"d":"0.00"}}]
[]
[7900,"1.2.3.14",null,"c)","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E165 = CHAR(37), F165*G165/100,F165*G165)","v":{"v":0,"d":"0.00"}}]
[]
[7901,"1.2.4","PSOH\r\nPS4.21","OCCUPATIONAL HEALTH & SAFETY"]
[]
[7902,"1.2.4.1",null,"General Safety (Time Related)","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E169 = CHAR(37), F169*G169/100,F169*G169)","v":{"v":0,"d":"0.00"}}]
[]
[7903,"1.2.4.2",null,"Training (time related) - Duration of training and detail of training to be specified","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E171 = CHAR(37), F171*G171/100,F171*G171)","v":{"v":0,"d":"0.00"}}]
[]
[10398,"1.2.4.3",null,"Contractors responsibility in terms of quality control and quality assurance, including method statements","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E173 = CHAR(37), F173*G173/100,F173*G173)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":33}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H154:H206)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 1 - PRELIMINARY AND GENERAL"]
[{"$nulls":7},"SECTION 1.3: OTHER PRELIMINARY AND GENERAL ITEMS"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[1802,"1.3",null,"OTHER PRELIMINARY AND GENERAL ITEMS"]
[]
[1803,"1.3.1","8.8","TEMPORARY WORKS"]
[]
[2529,"1.3.1.1",null,"Deal with traffic and maintain existing roads","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E215 = CHAR(37), F215*G215/100,F215*G215)","v":{"v":0,"d":"0.00"}}]
[]
[8622,"1.3.1.2","8.8.2\r\nSANS1921","Accommodation of traffic for construction vehicles entering and leaving the construction site","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E217 = CHAR(37), F217*G217/100,F217*G217)","v":{"v":0,"d":"0.00"}}]
[]
[8623,"1.3.1.3","8.8.4 (c)","Excavation by hand in soft material to expose suspected but unknown existing services.","m³",{"v":30,"d":"30.00"},{"v":0,"d":"0.00"},{"$f":"IF(E219 = CHAR(37), F219*G219/100,F219*G219)","v":{"v":0,"d":"0.00"}}]
[]
[20871,"1.3.1.4","PS 4.22","Access to Site and access road for the entire duration of the Contract","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E221 = CHAR(37), F221*G221/100,F221*G221)","v":{"v":0,"d":"0.00"}}]
[]
[1806,"1.3.2","PS 4.11.5\r\nPS 4.11","AS-BUILTS AND DOCUMENTATION"]
[]
[1794,null,null,"As-Built Survey, for:"]
[]
[2545,"1.3.2.1",null,"All pipelines and ancillary works ","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E227 = CHAR(37), F227*G227/100,F227*G227)","v":{"v":0,"d":"0.00"}}]
[]
[1798,"1.3.2.2",null,"Process units, chambers, channels, concrete structures, brickwork structures, pipework, valves, fittings and telemetry room, including  cables, conduits, manholes and other electrical equipment installed under the Contract.","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E229 = CHAR(37), F229*G229/100,F229*G229)","v":{"v":0,"d":"0.00"}}]
[]
[1799,"1.3.2.3",null,"Provision of full set of dimensioned marked up Record Drawings in A0 Hardcopy and Electronic PDF format","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E231 = CHAR(37), F231*G231/100,F231*G231)","v":{"v":0,"d":"0.00"}}]
[]
[20872,"1.3.3",null,"PRODUCTION OF A FULL SET OF ASBUILT DRAWINGS"]
[]
[20873,"1.3.3.1",null,"Asbuilt drawings of the entire Treatment Works site (Civil, Structural, Mechanical, Electrical, Instrumentation). This includes all applicable process units and structures/buildings on site. Including a consolidated and federated Revit Model of the entire works. ","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E235 = CHAR(37), F235*G235/100,F235*G235)","v":{"v":0,"d":"0.00"}}]
[]
[19983,"1.3.4","PSCOM","TRIAL OPERATIONAL PERIOD"]
[]
[19984,"1.3.4.1","PSCOM 7","Contractors Responsibility in terms of the Trial Operational Period","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E239 = CHAR(37), F239*G239/100,F239*G239)","v":{"v":0,"d":"0.00"}}]
[]
[19985,"1.3.5",null,"CONDITIONAL ASSESSMENTS"]
[]
[19986,"1.3.5.1",null,"Contractors Assessment of the entire site and compilation of structural defects and applicable remedial works","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E243 = CHAR(37), F243*G243/100,F243*G243)","v":{"v":0,"d":"0.00"}}]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H211:H243)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 1 - PRELIMINARY AND GENERAL"]
[{"$nulls":7},"SECTION 1.3: OTHER PRELIMINARY AND GENERAL ITEMS"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H244","v":{"v":0,"d":"0.00"}}]
[20885,"1.3.6",null,"EXPERIENTIAL TRAINING"]
[]
[20886,"1.3.6.1","PS4.20","Experiential training - local students","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E251 = CHAR(37), F251*G251/100,F251*G251)","v":{"v":0,"d":"0.00"}}]
[]
[22394,"1.3.7",null,"EQUIPMENT APPROVALS"]
[]
[22395,"1.3.7.1","PS1.4","Submission of associated documentation within 30 days of commencement of the Contract. Including monthly updates to the documentation","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E255 = CHAR(37), F255*G255/100,F255*G255)","v":{"v":0,"d":"0.00"}}]
[]
[24195,"1.3.8",null,"HAZOP"]
[]
[24196,"1.3.8.1",null,"HAZOP covering all scope of works within this Contract (Inclusive of the submission of HAZOP report & remedial works)","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E259 = CHAR(37), F259*G259/100,F259*G259)","v":{"v":0,"d":"0.00"}}]
[]
[24197,"1.3.9",null,"SHUTDOWNS/TIE-INS"]
[]
[24198,"1.3.9.1","PS4.4.8","Associated works for all shutdowns including the removal of sufficient existing pipe/structure to make way for new works, arranging shut-downs with eThekwini Municipality, cleaning and preparing the works for cutting, removal of blank flanges, dealing with all water (including that from leaking valves), preparing pipe ends for jointing, re-commissioning the pipeline/system and making good on site including all temporary supports. Inclusive of temporary supply systems to ensure the works remains operational. Note: Item to cover all planned shuts on the system for tie-ins","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E263 = CHAR(37), F263*G263/100,F263*G263)","v":{"v":0,"d":"0.00"}}]
[]
[25626,null,null,"APPOINTMENT OF A PROCESS ENGINEER"]
[]
[25627,null,null,"Appointment of a Professionally Registered Process Engineer. Responsibilities include process design support, performance monitoring, troubleshooting for all works undertaken on this contract","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E267 = CHAR(37), F267*G267/100,F267*G267)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":12}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H248:H279)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 1 - PRELIMINARY AND GENERAL"]
[{"$nulls":3},"SUMMARY OF SECTIONS"]
[null," ","SECTION","DESCRIPTION",{"$nulls":3},"AMOUNT\n(RAND)"]
[null,null,"1.1","SECTION 1.1: FIXED CHARGED ITEMS",{"$nulls":3},{"$f":"H105","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"1.2","SECTION 1.2: TIME RELATED ITEMS",{"$nulls":3},{"$f":"H207","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"1.3","SECTION 1.3: OTHER PRELIMINARY AND GENERAL ITEMS",{"$nulls":3},{"$f":"H280","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":53}
[null,null," Total Carried Forward To Summary Of Schedules"," Total Carried Forward To Summary Of Schedules",{"$nulls":3},{"$f":"SUM(H284:H341)","v":{"v":0,"d":"0.00"}}]

{"sheet":"Schedule 2","index":1,"n_rows":329,"n_cols":8,"rows_kept":329}
["Rate=G","SCHEDULE 2 - PROVISIONAL SUMS"]
[{"$nulls":7},"SECTION 2.1: PROVISIONAL SUMS"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[7273,"2.1","8.5","SUMS STATED PROVISIONALLY BY EMPLOYERS AGENT"]
[]
[7911,"2.1.1",null,"Provisional sum for concrete cube strength and durability tests ordered by the Employer’s Agent","Prov Sum",{"v":1,"d":"1.00"},{"v":100000,"d":"100,000.00"},{"v":100000,"d":"100,000.00"}]
[]
[7920,"2.1.2",null,"Overheads, charges and profit on above item","%",{"$f":"H6","v":{"v":100000,"d":"100,000.00"}},{"v":0,"d":"0.00"},{"$f":"IF(E8 = CHAR(37), F8*G8/100,F8*G8)","v":{"v":0,"d":"0.00"}}]
[]
[8227,"2.1.3",null,"Provisional Sum for non destructive testing of steel pipelines","Prov Sum",{"v":1,"d":"1.00"},{"v":100000,"d":"100,000.00"},{"v":100000,"d":"100,000.00"}]
[]
[8228,"2.1.4",null,"Overheads, charges and profit on above item","%",{"$f":"H10","v":{"v":100000,"d":"100,000.00"}},{"v":0,"d":"0.00"},{"$f":"IF(E12 = CHAR(37), F12*G12/100,F12*G12)","v":{"v":0,"d":"0.00"}}]
[]
[7921,"2.1.5","PS4.23, PCL","Provisional sum for employment CLO.","Prov Sum",{"v":1,"d":"1.00"},{"v":500000,"d":"500,000.00"},{"v":500000,"d":"500,000.00"}]
[]
[7922,"2.1.6",null,"Overheads, charges and profit on above item","%",{"$f":"H14","v":{"v":500000,"d":"500,000.00"}},{"v":0,"d":"0.00"},{"$f":"IF(E16 = CHAR(37), F16*G16/100,F16*G16)","v":{"v":0,"d":"0.00"}}]
[]
[7923,"2.1.7","PS4.11.4","Provisional sum for progress photographs/photographic record including drone imagery","Prov Sum",{"v":1,"d":"1.00"},{"v":35000,"d":"35,000.00"},{"v":35000,"d":"35,000.00"}]
[]
[7924,"2.1.8",null,"Overheads, charges and profit on above item","%",{"$f":"H18","v":{"v":35000,"d":"35,000.00"}},{"v":0,"d":"0.00"},{"$f":"IF(E20 = CHAR(37), F20*G20/100,F20*G20)","v":{"v":0,"d":"0.00"}}]
[]
[7925,"2.1.9",null,"Provisional sum for equipment for Employer’s Agent as directed","Prov Sum",{"v":1,"d":"1.00"},{"v":50000,"d":"50,000.00"},{"v":50000,"d":"50,000.00"}]
[]
[7926,"2.1.10",null,"Overheads, charges and profit on above item","%",{"$f":"H22","v":{"v":50000,"d":"50,000.00"}},{"v":0,"d":"0.00"},{"$f":"IF(E24 = CHAR(37), F24*G24/100,F24*G24)","v":{"v":0,"d":"0.00"}}]
[]
[8606,"2.1.11","PSD 8.3.7","Additional lateral support where ordered by the Engineer (provisional)","Prov Sum",{"v":1,"d":"1.00"},{"v":250000,"d":"250,000.00"},{"v":250000,"d":"250,000.00"}]
[]
[8607,"2.1.12",null,"Overheads, charges and profit on above item","%",{"$f":"H26","v":{"v":250000,"d":"250,000.00"}},{"v":0,"d":"0.00"},{"$f":"IF(E28 = CHAR(37), F28*G28/100,F28*G28)","v":{"v":0,"d":"0.00"}}]
[]
[8229,"2.1.13",null,"Provisional sum for additional specialised Engineering services as directed by the Employers Agent","Prov Sum",{"v":1,"d":"1.00"},{"v":500000,"d":"500,000.00"},{"v":500000,"d":"500,000.00"}]
[]
[8230,"2.1.14",null,"Overheads, charges and profit on above item","%",{"$f":"H30","v":{"v":500000,"d":"500,000.00"}},{"v":0,"d":"0.00"},{"$f":"IF(E32 = CHAR(37), F32*G32/100,F32*G32)","v":{"v":0,"d":"0.00"}}]
[]
[7912,"2.1.15",null,"Provisional sum for additional surveying as directed by the Employer’s Agent","Prov Sum",{"v":1,"d":"1.00"},{"v":75000,"d":"75,000.00"},{"v":75000,"d":"75,000.00"}]
[]
[7913,"2.1.16",null,"Overheads, charges and profit on above item","%",{"$f":"H34","v":{"v":75000,"d":"75,000.00"}},{"v":0,"d":"0.00"},{"$f":"IF(E36 = CHAR(37), F36*G36/100,F36*G36)","v":{"v":0,"d":"0.00"}}]
[]
[7315,"2.1.17",null,"Provisional sum for a weather station","Prov Sum",{"v":1,"d":"1.00"},{"v":25000,"d":"25,000.00"},{"v":25000,"d":"25,000.00"}]
[]
[7275,"2.1.18",null,"Overheads, charges and profit on above item","%",{"$f":"H38","v":{"v":25000,"d":"25,000.00"}},{"v":0,"d":"0.00"},{"$f":"IF(E40 = CHAR(37), F40*G40/100,F40*G40)","v":{"v":0,"d":"0.00"}}]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H4:H40)","v":{"v":1635000,"d":"1,635,000.00"}}]
[null,"SCHEDULE 2 - PROVISIONAL SUMS"]
[{"$nulls":7},"SECTION 2.1: PROVISIONAL SUMS"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H41","v":{"v":1635000,"d":"1,635,000.00"}}]
[18613,"2.1.19",null,"Provisional Sum for ancillary civil and structural remedial works","Prov Sum",{"v":1,"d":"1.00"},{"v":500000,"d":"500,000.00"},{"v":500000,"d":"500,000.00"}]
[]
[18614,"2.1.20",null,"Overheads, charges and profit on above item","%",{"$f":"H46","v":{"v":500000,"d":"500,000.00"}},{"v":0,"d":"0.00"},{"$f":"IF(E48 = CHAR(37), F48*G48/100,F48*G48)","v":{"v":0,"d":"0.00"}}]
[]
[19993,"2.1.21",null,"Provisional Sum for ancillary mechanical, electrical and instrumentation remedial works/equipment","Prov Sum",{"v":1,"d":"1.00"},{"v":500000,"d":"500,000.00"},{"v":500000,"d":"500,000.00"}]
[]
[19994,"2.1.22",null,"Overheads, charges and profit on above item","%",{"$f":"H50","v":{"v":500000,"d":"500,000.00"}},{"v":0,"d":"0.00"},{"$f":"IF(E52 = CHAR(37), F52*G52/100,F52*G52)","v":{"v":0,"d":"0.00"}}]
[]
[18922,"2.1.23",null,"Provisional sum for additional geotechnical investigations / monitoring","Prov Sum",{"v":1,"d":"1.00"},{"v":150000,"d":"150,000.00"},{"v":150000,"d":"150,000.00"}]
[]
[18923,"2.1.24",null,"Overheads, charges and profit on above item","%",{"$f":"H54","v":{"v":150000,"d":"150,000.00"}},{"v":0,"d":"0.00"},{"$f":"IF(E56 = CHAR(37), F56*G56/100,F56*G56)","v":{"v":0,"d":"0.00"}}]
[]
[24190,"2.1.25","PSCLR","Provisional Sum for colour coding painting of pipework","Prov Sum",{"v":1,"d":"1.00"},{"v":200000,"d":"200,000.00"},{"v":200000,"d":"200,000.00"}]
[]
[24191,"2.1.26",null,"Overheads, charges and profit on above item","%",{"$f":"H58","v":{"v":200000,"d":"200,000.00"}},{"v":0,"d":"0.00"},{"$f":"IF(E60 = CHAR(37), F60*G60/100,F60*G60)","v":{"v":0,"d":"0.00"}}]
[]
[25620,"2.1.27",null,"Provisional Sum for lock out boards","Prov Sum",{"v":1,"d":"1.00"},{"v":25000,"d":"25,000.00"},{"v":25000,"d":"25,000.00"}]
[]
[25621,"2.1.28",null,"Overheads, charges and profit on above item","%",{"$f":"H62","v":{"v":25000,"d":"25,000.00"}},{"v":0,"d":"0.00"},{"$f":"IF(E64 = CHAR(37), F64*G64/100,F64*G64)","v":{"v":0,"d":"0.00"}}]
[]
[25622,"2.1.29",null,"Provisional Sum for ISD Consultant","Prov Sum",{"v":1,"d":"1.00"},{"v":800000,"d":"800,000.00"},{"v":800000,"d":"800,000.00"}]
[]
[25623,"2.1.30",null,"Overheads, charges and profit on above item","%",{"$f":"H66","v":{"v":800000,"d":"800,000.00"}},{"v":0,"d":"0.00"},{"$f":"IF(E68 = CHAR(37), F68*G68/100,F68*G68)","v":{"v":0,"d":"0.00"}}]
[]
[25624,"2.1.31",null,"Provisional Sum for painting of walls, floors and ceilings as directed by the Engineer","Prov Sum",{"v":1,"d":"1.00"},{"v":200000,"d":"200,000.00"},{"v":200000,"d":"200,000.00"}]
[]
[25625,"2.1.32",null,"Overheads, charges and profit on above item","%",{"$f":"H70","v":{"v":200000,"d":"200,000.00"}},{"v":0,"d":"0.00"},{"$f":"IF(E72 = CHAR(37), F72*G72/100,F72*G72)","v":{"v":0,"d":"0.00"}}]
[]
[25628,"2.1.33",null,"Provisional Sum for Chlorine Building Extension","Prov Sum",{"v":1,"d":"1.00"},{"v":200000,"d":"200,000.00"},{"v":200000,"d":"200,000.00"}]
[]
[25629,"2.1.34",null,"Overheads, charges and profit on above item","%",{"$f":"H74","v":{"v":200000,"d":"200,000.00"}},{"v":0,"d":"0.00"},{"$f":"IF(E76 = CHAR(37), F76*G76/100,F76*G76)","v":{"v":0,"d":"0.00"}}]
[]
[26131,"2.1.35",null,"Provisional Sum for improvements to on site storage","Prov Sum",{"v":1,"d":"1.00"},{"v":5000000,"d":"5,000,000.00"},{"v":5000000,"d":"5,000,000.00"}]
[]
[26132,"2.1.36",null,"Overheads, charges and profit on above item","%",{"$f":"H78","v":{"v":5000000,"d":"5,000,000.00"}},{"v":0,"d":"0.00"},{"$f":"IF(E80 = CHAR(37), F80*G80/100,F80*G80)","v":{"v":0,"d":"0.00"}}]
[]
[]
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H45:H82)","v":{"v":9210000,"d":"9,210,000.00"}}]
[null,"SCHEDULE 2 - PROVISIONAL SUMS"]
[{"$nulls":7},"SECTION 2.2: DAYWORKS"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[7209,"2.2","SABS 1200A 8.7","DAYWORKS"]
[]
[7210,"2.2.1",null,"LABOUR"]
[]
[7211,"2.2.1.1",null,"Foreman","hr",{"v":30,"d":"30.00"},{"v":0,"d":"0.00"},{"$f":"IF(E91 = CHAR(37), F91*G91/100,F91*G91)","v":{"v":0,"d":"0.00"}}]
[]
[7214,"2.2.1.2",null,"Semi-skilled","hr",{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"$f":"IF(E93 = CHAR(37), F93*G93/100,F93*G93)","v":{"v":0,"d":"0.00"}}]
[]
[7215,"2.2.1.3",null,"Unskilled","hr",{"v":200,"d":"200.00"},{"v":0,"d":"0.00"},{"$f":"IF(E95 = CHAR(37), F95*G95/100,F95*G95)","v":{"v":0,"d":"0.00"}}]
[]
[7216,"2.2.1.4",null,"Surveyor with transport, instruments and labour","hr",{"v":40,"d":"40.00"},{"v":0,"d":"0.00"},{"$f":"IF(E97 = CHAR(37), F97*G97/100,F97*G97)","v":{"v":0,"d":"0.00"}}]
[]
[7217,"2.2.2",null,"PLANT"]
[]
[7218,"2.2.2.1",null,"CAT 930 (75kW) or similar including establishment and de-establishment ","hr",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E101 = CHAR(37), F101*G101/100,F101*G101)","v":{"v":0,"d":"0.00"}}]
[]
[7219,"2.2.2.2",null,"Other (Contractor to specify)","hr",{"v":20,"d":"20.00"},{"v":0,"d":"0.00"},{"$f":"IF(E103 = CHAR(37), F103*G103/100,F103*G103)","v":{"v":0,"d":"0.00"}}]
[]
[7220,null,null,"Bulldozer with ripper:"]
[]
[7223,"2.2.2.3",null,"CAT D8 or similar","hr",{"v":30,"d":"30.00"},{"v":0,"d":"0.00"},{"$f":"IF(E107 = CHAR(37), F107*G107/100,F107*G107)","v":{"v":0,"d":"0.00"}}]
[]
[7225,null,null,"Motor Grader:"]
[]
[7226,"2.2.2.4",null,"110 kW","hr",{"v":30,"d":"30.00"},{"v":0,"d":"0.00"},{"$f":"IF(E111 = CHAR(37), F111*G111/100,F111*G111)","v":{"v":0,"d":"0.00"}}]
[]
[7227,"2.2.2.5",null,"Other (Contractor to specify)","hr",{"v":20,"d":"20.00"},{"v":0,"d":"0.00"},{"$f":"IF(E113 = CHAR(37), F113*G113/100,F113*G113)","v":{"v":0,"d":"0.00"}}]
[]
[7228,null,null,"Tip Truck:"]
[]
[7230,"2.2.2.6",null,"10m³","hr",{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"$f":"IF(E117 = CHAR(37), F117*G117/100,F117*G117)","v":{"v":0,"d":"0.00"}}]
[]
[8244,"2.2.2.7",null,"6m³","hr",{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"$f":"IF(E119 = CHAR(37), F119*G119/100,F119*G119)","v":{"v":0,"d":"0.00"}}]
[]
[7231,"2.2.2.8",null,"Other (Contractor to specify)","hr",{"v":20,"d":"20.00"},{"v":0,"d":"0.00"},{"$f":"IF(E121 = CHAR(37), F121*G121/100,F121*G121)","v":{"v":0,"d":"0.00"}}]
[]
[7232,null,null,"Backactor:"]
[]
[7233,"2.2.2.9",null,"100kW, 23 ton","hr",{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"$f":"IF(E125 = CHAR(37), F125*G125/100,F125*G125)","v":{"v":0,"d":"0.00"}}]
[]
[7234,"2.2.2.10",null,"30 ton","hr",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E127 = CHAR(37), F127*G127/100,F127*G127)","v":{"v":0,"d":"0.00"}}]
[]
[7235,"2.2.2.11",null,"TLB","hr",{"v":80,"d":"80.00"},{"v":0,"d":"0.00"},{"$f":"IF(E129 = CHAR(37), F129*G129/100,F129*G129)","v":{"v":0,"d":"0.00"}}]
[]
[7236,"2.2.2.12",null,"Other (Contractor to specify)","hr",{"v":20,"d":"20.00"},{"v":0,"d":"0.00"},{"$f":"IF(E131 = CHAR(37), F131*G131/100,F131*G131)","v":{"v":0,"d":"0.00"}}]
[]
[7237,null,null,"Compactors:"]
[]
[7238,"2.2.2.13",null,"Self propelled vibrating roller, 9 ton","hr",{"v":20,"d":"20.00"},{"v":0,"d":"0.00"},{"$f":"IF(E135 = CHAR(37), F135*G135/100,F135*G135)","v":{"v":0,"d":"0.00"}}]
[]
[7239,"2.2.2.14",null,"Bomag 60 or similar","hr",{"v":20,"d":"20.00"},{"v":0,"d":"0.00"},{"$f":"IF(E137 = CHAR(37), F137*G137/100,F137*G137)","v":{"v":0,"d":"0.00"}}]
[]
[7240,"2.2.2.15",null,"Plate compactor","hr",{"v":20,"d":"20.00"},{"v":0,"d":"0.00"},{"$f":"IF(E139 = CHAR(37), F139*G139/100,F139*G139)","v":{"v":0,"d":"0.00"}}]
[]
[7241,"2.2.2.16",null,"Other (Contractor to specify)","hr",{"v":20,"d":"20.00"},{"v":0,"d":"0.00"},{"$f":"IF(E141 = CHAR(37), F141*G141/100,F141*G141)","v":{"v":0,"d":"0.00"}}]
[]
[7242,"2.2.2.17",null,"Pneumatic Roller","hr",{"v":20,"d":"20.00"},{"v":0,"d":"0.00"},{"$f":"IF(E143 = CHAR(37), F143*G143/100,F143*G143)","v":{"v":0,"d":"0.00"}}]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H87:H143)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 2 - PROVISIONAL SUMS"]
[{"$nulls":7},"SECTION 2.2: DAYWORKS"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H144","v":{"v":0,"d":"0.00"}}]
[7243,null,null,"Water Tankers:"]
[]
[7245,"2.2.2.18",null,"Water Tanker 9000 litres","hr",{"v":100,"d":"100.00"},{"v":0,"d":"0.00"},{"$f":"IF(E151 = CHAR(37), F151*G151/100,F151*G151)","v":{"v":0,"d":"0.00"}}]
[]
[7246,null,null,"Self propelled Crane:"]
[]
[7247,"2.2.2.19",null,"20 Tonne","hr",{"v":20,"d":"20.00"},{"v":0,"d":"0.00"},{"$f":"IF(E155 = CHAR(37), F155*G155/100,F155*G155)","v":{"v":0,"d":"0.00"}}]
[]
[7249,"2.2.2.20",null,"Generator and Breaker 5KVA","hr",{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"$f":"IF(E157 = CHAR(37), F157*G157/100,F157*G157)","v":{"v":0,"d":"0.00"}}]
[]
[7250,"2.2.2.21",null,"Water/Sludge Pump 50mm","hr",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E159 = CHAR(37), F159*G159/100,F159*G159)","v":{"v":0,"d":"0.00"}}]
[]
[7251,null,null,"Welding Equipment:"]
[]
[7252,"2.2.2.22",null,"Heavy duty, self powered welding machine 400A","hr",{"v":20,"d":"20.00"},{"v":0,"d":"0.00"},{"$f":"IF(E163 = CHAR(37), F163*G163/100,F163*G163)","v":{"v":0,"d":"0.00"}}]
[]
[7253,"2.2.2.23",null,"Welder ( Coded) with assistant","hr",{"v":20,"d":"20.00"},{"v":0,"d":"0.00"},{"$f":"IF(E165 = CHAR(37), F165*G165/100,F165*G165)","v":{"v":0,"d":"0.00"}}]
[]
[7254,null,null,"Various Other:"]
[]
[7255,"2.2.2.24",null,"Compressor 400 cuft/min - with 2 breakers","hr",{"v":30,"d":"30.00"},{"v":0,"d":"0.00"},{"$f":"IF(E169 = CHAR(37), F169*G169/100,F169*G169)","v":{"v":0,"d":"0.00"}}]
[]
[7257,"2.2.2.25",null,"Electric breaker - single phase","day",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E171 = CHAR(37), F171*G171/100,F171*G171)","v":{"v":0,"d":"0.00"}}]
[]
[7258,"2.2.2.26",null,"Angle Grinder - 230mm","day",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E173 = CHAR(37), F173*G173/100,F173*G173)","v":{"v":0,"d":"0.00"}}]
[]
[7259,"2.2.2.27",null,"Pneumatic Hammer Drill - 1500Watt","day",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E175 = CHAR(37), F175*G175/100,F175*G175)","v":{"v":0,"d":"0.00"}}]
[]
[7260,"2.2.2.28",null,"Concrete mixer - 360l capacity","day",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E177 = CHAR(37), F177*G177/100,F177*G177)","v":{"v":0,"d":"0.00"}}]
[]
[7261,"2.2.2.29",null,"7 Tonne flat bed with mounted crane and driver","hr",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E179 = CHAR(37), F179*G179/100,F179*G179)","v":{"v":0,"d":"0.00"}}]
[]
[7262,"2.2.2.30",null,"1 Tonne LDV with driver","km",{"v":200,"d":"200.00"},{"v":0,"d":"0.00"},{"$f":"IF(E181 = CHAR(37), F181*G181/100,F181*G181)","v":{"v":0,"d":"0.00"}}]
[]
[7263,"2.2.2.31",null,"Tractor 30 kW or similar","hr",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E183 = CHAR(37), F183*G183/100,F183*G183)","v":{"v":0,"d":"0.00"}}]
[]
[7212,"2.2.2.32",null,"3 Disk Plow","hr",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E185 = CHAR(37), F185*G185/100,F185*G185)","v":{"v":0,"d":"0.00"}}]
[]
[7213,"2.2.3",null,"MATERIALS"]
[]
[7264,"2.2.3.1",null,"Sand (building)","m³",{"v":100,"d":"100.00"},{"v":0,"d":"0.00"},{"$f":"IF(E189 = CHAR(37), F189*G189/100,F189*G189)","v":{"v":0,"d":"0.00"}}]
[]
[7931,"2.2.3.2",null,"Sand (river)","m³",{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"$f":"IF(E191 = CHAR(37), F191*G191/100,F191*G191)","v":{"v":0,"d":"0.00"}}]
[]
[7265,"2.2.3.3",null,"50kg pocket of Cement","No.",{"v":30,"d":"30.00"},{"v":0,"d":"0.00"},{"$f":"IF(E193 = CHAR(37), F193*G193/100,F193*G193)","v":{"v":0,"d":"0.00"}}]
[]
[7266,"2.2.3.4",null,"Dump Rock 150mm","m³",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E195 = CHAR(37), F195*G195/100,F195*G195)","v":{"v":0,"d":"0.00"}}]
[]
[7267,"2.2.3.5",null,"Crusher Run 28mm","m³",{"v":20,"d":"20.00"},{"v":0,"d":"0.00"},{"$f":"IF(E197 = CHAR(37), F197*G197/100,F197*G197)","v":{"v":0,"d":"0.00"}}]
[]
[7268,"2.2.3.6",null,"G5 material","m³",{"v":20,"d":"20.00"},{"v":0,"d":"0.00"},{"$f":"IF(E199 = CHAR(37), F199*G199/100,F199*G199)","v":{"v":0,"d":"0.00"}}]
[]
[7932,"2.2.3.7",null,"G2 material","m³",{"v":20,"d":"20.00"},{"v":0,"d":"0.00"},{"$f":"IF(E201 = CHAR(37), F201*G201/100,F201*G201)","v":{"v":0,"d":"0.00"}}]
[]
[8245,"2.2.3.8",null,"Provisional sum for cost of other materials ","Prov Sum",{"v":1,"d":"1.00"},{"v":50000,"d":"50,000.00"},{"v":50000,"d":"50,000.00"}]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H148:H203)","v":{"v":50000,"d":"50,000.00"}}]
[null,"SCHEDULE 2 - PROVISIONAL SUMS"]
[{"$nulls":7},"SECTION 2.2: DAYWORKS"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H204","v":{"v":50000,"d":"50,000.00"}}]
[7269,null,null,"Other (To be specified by Contractor, a breakdown to be attached)"]
[]
[7270,null,null,"a)"]
[]
[7271,null,null,"b)"]
[]
[7272,null,null,"c)"]
{"$rows_empty":51}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H208:H266)","v":{"v":50000,"d":"50,000.00"}}]
[null,"SCHEDULE 2 - PROVISIONAL SUMS"]
[{"$nulls":3},"SUMMARY OF SECTIONS"]
[null," ","SECTION","DESCRIPTION",{"$nulls":3},"AMOUNT\n(RAND)"]
[null,null,"2.1","SECTION 2.1: PROVISIONAL SUMS",{"$nulls":3},{"$f":"H83","v":{"v":9210000,"d":"9,210,000.00"}}]
[]
[null,null,"2.2","SECTION 2.2: DAYWORKS",{"$nulls":3},{"$f":"H267","v":{"v":50000,"d":"50,000.00"}}]
{"$rows_empty":55}
[null,null," Total Carried Forward To Summary Of Schedules"," Total Carried Forward To Summary Of Schedules",{"$nulls":3},{"$f":"SUM(H271:H328)","v":{"v":9260000,"d":"9,260,000.00"}}]

{"sheet":"Schedule 3","index":2,"n_rows":679,"n_cols":8,"rows_kept":679}
["Rate=G","SCHEDULE 3 - HEAD OF WORKS"]
[{"$nulls":7},"SECTION 3: HEAD OF WORKS "]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[25379,"3.1",null,"SECTION 3: HEAD OF WORKS \r\nEARTHWORKS"]
[]
[25380,"3.1.1","SANS 1200D","EARTHWORKS "]
[]
[25463,"3.1.1.1","8.3.3","Excavate by hand around existing Mixing structure and/or existing offtake to works to prove existing pipelines for proposed bypass","m³",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E8 = CHAR(37), F8*G8/100,F8*G8)","v":{"v":0,"d":"0.00"}}]
[]
[25464,"3.1.2","SANS 1200DB\r\nPSDB","EARTHWORKS (PIPE TRENCHES)"]
[]
[25465,"3.1.2.1","8.3.5","Excavate by hand for proofing of existing Rising main","m³",{"v":30,"d":"30.00"},{"v":0,"d":"0.00"},{"$f":"IF(E12 = CHAR(37), F12*G12/100,F12*G12)","v":{"v":0,"d":"0.00"}}]
[]
[25466,"3.1.2.2","8.3.2 a","Remove topsoil to nominal depth of 150mm, stockpile and maintain ","m²",{"v":60,"d":"60.00"},{"v":0,"d":"0.00"},{"$f":"IF(E14 = CHAR(37), F14*G14/100,F14*G14)","v":{"v":0,"d":"0.00"}}]
[]
[25467,"3.1.2.3","8.3.6","Topsoil from stockpile provided for under item 3.2.2","m²",{"v":60,"d":"60.00"},{"v":0,"d":"0.00"},{"$f":"IF(E16 = CHAR(37), F16*G16/100,F16*G16)","v":{"v":0,"d":"0.00"}}]
[]
[25468,"3.1.2.4","8.3.7","Supply and lay approved grassing as specified in the EMP","m²",{"v":60,"d":"60.00"},{"v":0,"d":"0.00"},{"$f":"IF(E18 = CHAR(37), F18*G18/100,F18*G18)","v":{"v":0,"d":"0.00"}}]
[]
[25469,null,"8.3.2\r\nPSDB","Excavate in all materials for pipe trench up to DN500 pipe, backfill, compact & dispose of surplus material for depths: "]
[]
[25470,null,null,"Over and up to:"]
[]
[25471,"3.1.2.5",null,"0.0 - 0.5m","m",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E24 = CHAR(37), F24*G24/100,F24*G24)","v":{"v":0,"d":"0.00"}}]
[]
[25472,"3.1.2.6",null,"0.51 - 1.0m","m",{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"$f":"IF(E26 = CHAR(37), F26*G26/100,F26*G26)","v":{"v":0,"d":"0.00"}}]
[]
[25473,"3.1.2.7",null,"1.01 - 2m","m",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E28 = CHAR(37), F28*G28/100,F28*G28)","v":{"v":0,"d":"0.00"}}]
[]
[25474,"3.1.2.8","8.3.2","Extra over items 3.2.5 to 3.2.7 for excavation in hard rock","m³",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E30 = CHAR(37), F30*G30/100,F30*G30)","v":{"v":0,"d":"0.00"}}]
[]
[25475,"3.1.2.9","8.3.3.4(b)","Overhaul for spoil material under item 3.2.5 to 3.2.7 as instructed by the Engineer","m³.km",{"v":15,"d":"15.00"},{"v":0,"d":"0.00"},{"$f":"IF(E32 = CHAR(37), F32*G32/100,F32*G32)","v":{"v":0,"d":"0.00"}}]
[]
[25476,"3.1.2.10",null,"Extra over items 3.2.1 to 3.2.3 for saw cutting of asphalt surface","m",{"v":80,"d":"80.00"},{"v":0,"d":"0.00"},{"$f":"IF(E34 = CHAR(37), F34*G34/100,F34*G34)","v":{"v":0,"d":"0.00"}}]
[]
[25477,null,"8.3.5","Services that intersect or adjoin a trench"]
[]
[25478,"3.1.2.11",null,"a) Services that intersect a trench","No.",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E38 = CHAR(37), F38*G38/100,F38*G38)","v":{"v":0,"d":"0.00"}}]
[]
[25479,"3.1.2.12",null,"b)  Services that adjoin a trench","m",{"v":40,"d":"40.00"},{"v":0,"d":"0.00"},{"$f":"IF(E40 = CHAR(37), F40*G40/100,F40*G40)","v":{"v":0,"d":"0.00"}}]
[]
[25480,"3.1.3","SANS 1200M","ROAD WORKS"]
[]
[25481,null,null,"Re-instatement of road surfaces, including all layer works as detailed below:"]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H4:H44)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 3 - HEAD OF WORKS"]
[{"$nulls":7},"SECTION 3: HEAD OF WORKS "]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H45","v":{"v":0,"d":"0.00"}}]
[25482,"3.1.3.1","8.3.6.1","40mm asphalt surfacing including tack coat","m²",{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"$f":"IF(E50 = CHAR(37), F50*G50/100,F50*G50)","v":{"v":0,"d":"0.00"}}]
[]
[25483,"3.1.3.2","8.3.6.1","150mm thick G7  sub base compacted to 98% ModAASHO","m²",{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"$f":"IF(E52 = CHAR(37), F52*G52/100,F52*G52)","v":{"v":0,"d":"0.00"}}]
[]
[25484,"3.1.3.3","8.3.6.1","150mm thick G7  sub base compacted to 95% ModAASHO","m²",{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"$f":"IF(E54 = CHAR(37), F54*G54/100,F54*G54)","v":{"v":0,"d":"0.00"}}]
[]
[25485,"3.1.3.4",null,"Compaction of pipe trenches in gravel road to 90% mod AASHTO","m³",{"v":35,"d":"35.00"},{"v":0,"d":"0.00"},{"$f":"IF(E56 = CHAR(37), F56*G56/100,F56*G56)","v":{"v":0,"d":"0.00"}}]
[]
[25486,"3.1.3.5",null,"Replacement of kerbs to roadway including concrete support","m",{"v":70,"d":"70.00"},{"v":0,"d":"0.00"},{"$f":"IF(E58 = CHAR(37), F58*G58/100,F58*G58)","v":{"v":0,"d":"0.00"}}]
[]
[25487,"3.1.4",null,"BEDDING (PIPE)"]
[]
[25488,null,null,"Selected granular material for Class C bedding and fill where ordered, obtained from:"]
[]
[25489,"3.1.4.1","8.2.2.1","Trench excavations","m³",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E64 = CHAR(37), F64*G64/100,F64*G64)","v":{"v":0,"d":"0.00"}}]
[]
[25490,"3.1.4.2","8.2.2.3","Commercial sources","m³",{"v":90,"d":"90.00"},{"v":0,"d":"0.00"},{"$f":"IF(E66 = CHAR(37), F66*G66/100,F66*G66)","v":{"v":0,"d":"0.00"}}]
[]
[25491,"3.1.5","SANS 1200L\r\nPSL","MEDIUM PRESSURE PIPELINES"]
[]
[25492,null,null,"Note: The tendered prices for pipes, valves & specials to include for the cost of necessary couplings, sockets, or flange jointing material scarfing, cutting, welding, jointing and repairs to coatings and linings as necessary. This section allows provisional quantities, however final measurement will depend on agreed option for tie-in"]
[]
[25493,null,"8.2.1\r\nPSL","Supply, lay, bed & test pipes complete with all field welds and repairs to coating and lining the following grade X42 Steel (Plain Ended, suitable for VJ) epoxy coated and lined pipes to specification, including the manufacture, coating, lining, repair, installation and testing complete of all bends up to 5 deg. : "]
[]
[25494,"3.1.5.1",null,"DN400mm OD, 4,5mm wall thickness epoxy coated and lined X42 steel site run pipeline (VJ jointed) wrapped with 55% overlap 1250 micron Denso Ultraflex (or similar approved)","m",{"v":20,"d":"20.00"},{"v":0,"d":"0.00"},{"$f":"IF(E74 = CHAR(37), F74*G74/100,F74*G74)","v":{"v":0,"d":"0.00"}}]
[]
[]
[]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H49:H78)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 3 - HEAD OF WORKS"]
[{"$nulls":7},"SECTION 3: HEAD OF WORKS "]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H79","v":{"v":0,"d":"0.00"}}]
[25495,"3.1.5.2",null,"DN400 VJ coupling to suit DN400mm OD 4,5mm X42 steel pipe, with central register, together with petromastic, petrolatum, and topping tape (or similar approved)","No.",{"v":8,"d":"8.00"},{"v":0,"d":"0.00"},{"$f":"IF(E84 = CHAR(37), F84*G84/100,F84*G84)","v":{"v":0,"d":"0.00"}}]
[]
[25496,null,"8.2.5\r\nPSL ","Extra over item 3.5.1 for supplying, laying & bedding of the following DN400mm OD 4,5mm wall thickness steel coated and lined Grade X42 special bends and reducers to  specification including welding and repairs to coatings and linings, all bends and reducers to include DN200 flanged stub complete with blank flange and ball valve and precast manhole as detailed for inspection purposes. All ends prepared for VJ coupling wrapped with 1250 micron Denso Ultraflex (or similar approved) at 55% overlap:"]
[]
[25497,"3.1.5.3",null,">5° - 11¼° long radius bend","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E88 = CHAR(37), F88*G88/100,F88*G88)","v":{"v":0,"d":"0.00"}}]
[]
[25498,"3.1.5.4",null,">11¼° - 22½° long radius bend","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E90 = CHAR(37), F90*G90/100,F90*G90)","v":{"v":0,"d":"0.00"}}]
[]
[25499,"3.1.5.5",null,">22½° - 45° long radius  bend","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E92 = CHAR(37), F92*G92/100,F92*G92)","v":{"v":0,"d":"0.00"}}]
[]
[25500,"3.1.5.6",null,">45° - 90° long radius bend","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E94 = CHAR(37), F94*G94/100,F94*G94)","v":{"v":0,"d":"0.00"}}]
[]
[25501,"3.1.5.7",null,"DN500mm OD, 4,5mm wall thickness epoxy coated and lined X42 steel site run pipeline (VJ jointed) wrapped with 55% overlap 1250 micron Denso Ultraflex (or similar approved)","m",{"v":40,"d":"40.00"},{"v":0,"d":"0.00"},{"$f":"IF(E96 = CHAR(37), F96*G96/100,F96*G96)","v":{"v":0,"d":"0.00"}}]
[]
[25502,"3.1.5.8",null,"DN500 VJ coupling to suit DN500mm OD 4,5mm X42 steel pipe, with central register, together with petromastic, petrolatum, and topping tape (or similar approved)","No.",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E98 = CHAR(37), F98*G98/100,F98*G98)","v":{"v":0,"d":"0.00"}}]
[]
[25503,null,"8.2.5\r\nPSL ","Extra over item 3.5.7 for supplying, laying & bedding of the following DN500mm OD 4,5mm wall thickness steel coated and lined Grade X42 special bends and reducers to  specification including welding and repairs to coatings and linings, all bends and reducers to include DN200 flanged stub complete with blank flange and ball valve and precast manhole as detailed for inspection purposes. All ends prepared for VJ coupling wrapped with 1250 micron Denso Ultraflex (or similar approved) at 55% overlap:"]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H83:H101)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 3 - HEAD OF WORKS"]
[{"$nulls":7},"SECTION 3: HEAD OF WORKS "]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H102","v":{"v":0,"d":"0.00"}}]
[25504,"3.1.5.9",null,">5° - 11¼° long radius bend","No.",{"v":3,"d":"3.00"},{"v":0,"d":"0.00"},{"$f":"IF(E107 = CHAR(37), F107*G107/100,F107*G107)","v":{"v":0,"d":"0.00"}}]
[]
[25505,"3.1.5.10",null,">11¼° - 22½° long radius bend","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E109 = CHAR(37), F109*G109/100,F109*G109)","v":{"v":0,"d":"0.00"}}]
[]
[25506,"3.1.5.11",null,">22½° - 45° long radius  bend","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E111 = CHAR(37), F111*G111/100,F111*G111)","v":{"v":0,"d":"0.00"}}]
[]
[25507,"3.1.5.12",null,">45° - 90° long radius bend","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E113 = CHAR(37), F113*G113/100,F113*G113)","v":{"v":0,"d":"0.00"}}]
[]
[25604,null,null,"OFFTAKE (ISOLATION AND METER) CHAMBER AND ROAD CROSSING (Ref drawing 60398/38, 60398/39)"]
[]
[25508,"3.1.6","SANS 1200D\r\nPSD","EARTHWORKS"]
[]
[25509,"3.1.6.1","8.3.1.2","Remove topsoil to a normal depth of 150mm stockpile & maintain","m²",{"v":80,"d":"80.00"},{"v":0,"d":"0.00"},{"$f":"IF(E119 = CHAR(37), F119*G119/100,F119*G119)","v":{"v":0,"d":"0.00"}}]
[]
[25510,"3.1.6.2","8.3.3","Restricted excavation in all materials irrespective of depth for chambers","m³",{"v":100,"d":"100.00"},{"v":0,"d":"0.00"},{"$f":"IF(E121 = CHAR(37), F121*G121/100,F121*G121)","v":{"v":0,"d":"0.00"}}]
[]
[25511,"3.1.6.3","8.3.6","Overhaul for spoil material under item 3.6.1.1/2 as instructed by the Engineer","m³.km",{"v":20,"d":"20.00"},{"v":0,"d":"0.00"},{"$f":"IF(E123 = CHAR(37), F123*G123/100,F123*G123)","v":{"v":0,"d":"0.00"}}]
[]
[25512,"3.1.7","SANS 1200D\r\nPSD","FINISHES",null,{"v":160,"d":"160.00"}]
[]
[25513,"3.1.7.1","8.3.10","Topsoiling from stockpile under item 3.6.1.1","m²",{"v":70,"d":"70.00"},{"v":0,"d":"0.00"},{"$f":"IF(E127 = CHAR(37), F127*G127/100,F127*G127)","v":{"v":0,"d":"0.00"}}]
[]
[25514,"3.1.7.2","8.3.11","Supply and lay approved grass sodding as specified in the EMP","m²",{"v":70,"d":"70.00"},{"v":0,"d":"0.00"},{"$f":"IF(E129 = CHAR(37), F129*G129/100,F129*G129)","v":{"v":0,"d":"0.00"}}]
[]
[25515,null,"SANS 1200G\r\nPSG","CONCRETE WORKS (STRUCTURAL)"]
[]
[25516,"3.1.8","8.1.1","FORMWORK"]
[]
[25517,null,null,"Supply, install and remove upon completion all necessary formwork shutters, propping, scaffold support work, ledges, soldiers, keys, wedges and ferrels complete.  Rate inclusive of boxing out for pipework and manholes."]
[]
[25518,null,"8.2.2","Smooth vertical to chambers"]
[]
[25519,"3.1.8.1",null,"Vertical wall surfaces to chambers","m²",{"v":70,"d":"70.00"},{"v":0,"d":"0.00"},{"$f":"IF(E139 = CHAR(37), F139*G139/100,F139*G139)","v":{"v":0,"d":"0.00"}}]
[]
[25520,null,"8.2.5","Narrow Widths to chambers not exceeding 250mm"]
[]
[25521,"3.1.8.2",null,"External floor slab","m",{"v":16,"d":"16.00"},{"v":0,"d":"0.00"},{"$f":"IF(E143 = CHAR(37), F143*G143/100,F143*G143)","v":{"v":0,"d":"0.00"}}]
[]
[25522,"3.1.8.3",null,"25 x 25mm extra over for chamfer to all exposed edges","m",{"v":15,"d":"15.00"},{"v":0,"d":"0.00"},{"$f":"IF(E145 = CHAR(37), F145*G145/100,F145*G145)","v":{"v":0,"d":"0.00"}}]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H106:H146)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 3 - HEAD OF WORKS"]
[{"$nulls":7},"SECTION 3: HEAD OF WORKS "]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H147","v":{"v":0,"d":"0.00"}}]
[25523,null,"8.2.2","Smooth horizontal soffits to chambers including propped to:"]
[]
[25524,"3.1.8.4",null,"Soffit for roof slab 2.4m","m²",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E154 = CHAR(37), F154*G154/100,F154*G154)","v":{"v":0,"d":"0.00"}}]
[]
[25525,null,null,"Rough vertical to thrust blocks"]
[]
[25526,"3.1.8.5",null,"Side walls of thrust blocks","m²",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E158 = CHAR(37), F158*G158/100,F158*G158)","v":{"v":0,"d":"0.00"}}]
[]
[25527,null,null,"Narrow widths to road crossing pipe protection slab"]
[]
[25528,"3.1.8.6","8.2.5","Road crossing pipe protection slab (internal to 300mm width)","m",{"v":20,"d":"20.00"},{"v":0,"d":"0.00"},{"$f":"IF(E162 = CHAR(37), F162*G162/100,F162*G162)","v":{"v":0,"d":"0.00"}}]
[]
[25529,"3.1.8.7","8.2.5","Road crossing pipe protection slab (external to 150mm width)","m",{"v":20,"d":"20.00"},{"v":0,"d":"0.00"},{"$f":"IF(E164 = CHAR(37), F164*G164/100,F164*G164)","v":{"v":0,"d":"0.00"}}]
[]
[25530,"3.1.9","8.1.2","REINFORCEMENT"]
[]
[25531,"3.1.9.1","8.3.1","High tensile steel reinforcement of all diameters between 8mm and 25mm in chamber floors, walls and roofs.","t",{"v":3,"d":"3.00"},{"v":0,"d":"0.00"},{"$f":"IF(E168 = CHAR(37), F168*G168/100,F168*G168)","v":{"v":0,"d":"0.00"}}]
[]
[25532,"3.1.9.2","8.3.1","MS reinforcement of all diameters between 8mm and 32mm","t",{"v":0.1,"d":"0.10"},{"v":0,"d":"0.00"},{"$f":"IF(E170 = CHAR(37), F170*G170/100,F170*G170)","v":{"v":0,"d":"0.00"}}]
[]
[25533,"3.1.9.3","8.3.2","Mesh ref 888","m²",{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"$f":"IF(E172 = CHAR(37), F172*G172/100,F172*G172)","v":{"v":0,"d":"0.00"}}]
[]
[25534,"3.1.9.4",null,"25mm galvanised round bar dowels 500mm long cast halfway into road protection slab (inner) and coated with debonding agent for outer slab (300 centres)","No.",{"v":90,"d":"90.00"},{"v":0,"d":"0.00"},{"$f":"IF(E174 = CHAR(37), F174*G174/100,F174*G174)","v":{"v":0,"d":"0.00"}}]
[]
[25535,"3.1.10","8.1.3","CONCRETE"]
[]
[25607,"3.1.10.1","PSG 5.5.3.2","Concrete Mix Designs","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E178 = CHAR(37), F178*G178/100,F178*G178)","v":{"v":0,"d":"0.00"}}]
[]
[25536,"3.1.10.2","8.4.2","Blinding layer 40mm thick in grade 15/19 concrete to chambers","m²",{"v":16,"d":"16.00"},{"v":0,"d":"0.00"},{"$f":"IF(E180 = CHAR(37), F180*G180/100,F180*G180)","v":{"v":0,"d":"0.00"}}]
[]
[25537,null,"8.4.3","Grade 25/19 concrete in chambers"]
[]
[25538,"3.1.10.3",null,"Chamber","m³",{"v":17,"d":"17.00"},{"v":0,"d":"0.00"},{"$f":"IF(E184 = CHAR(37), F184*G184/100,F184*G184)","v":{"v":0,"d":"0.00"}}]
[]
[25539,null,"8.4.3","Grade 25/19 concrete"]
[]
[25540,"3.1.10.4",null,"Road crossing pipe protection slab","m³",{"v":8,"d":"8.00"},{"v":0,"d":"0.00"},{"$f":"IF(E188 = CHAR(37), F188*G188/100,F188*G188)","v":{"v":0,"d":"0.00"}}]
[]
[25541,null,"8.4.3","Grade 15/19 concrete "]
[]
[25542,"3.1.10.5",null,"For thrust blocks/anchor blocks/valve supports","m³",{"v":15,"d":"15.00"},{"v":0,"d":"0.00"},{"$f":"IF(E192 = CHAR(37), F192*G192/100,F192*G192)","v":{"v":0,"d":"0.00"}}]
[]
[25543,"3.1.11",null,"UNFORMED SURFACE FINISHES"]
[]
[25544,null,"8.4.4 (b)","Steel float finish"]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H151:H196)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 3 - HEAD OF WORKS"]
[{"$nulls":7},"SECTION 3: HEAD OF WORKS "]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H197","v":{"v":0,"d":"0.00"}}]
[25545,"3.1.11.1",null,"Chamber Floor Slabs","m²",{"v":9,"d":"9.00"},{"v":0,"d":"0.00"},{"$f":"IF(E202 = CHAR(37), F202*G202/100,F202*G202)","v":{"v":0,"d":"0.00"}}]
[]
[25546,"3.1.11.2",null,"Chamber Roof Slabs","m²",{"v":12,"d":"12.00"},{"v":0,"d":"0.00"},{"$f":"IF(E204 = CHAR(37), F204*G204/100,F204*G204)","v":{"v":0,"d":"0.00"}}]
[]
[25547,"3.1.11.3",null,"Road crossing pipe protection slab","m²",{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"$f":"IF(E206 = CHAR(37), F206*G206/100,F206*G206)","v":{"v":0,"d":"0.00"}}]
[]
[25608,"3.1.12","PSG 5.5.8\r\nPSG 8.4.7","CURING AND PROTECTION"]
[]
[25609,"3.1.12.1",null,"Wall slab","m²",{"v":70,"d":"70.00"},{"v":0,"d":"0.00"},{"$f":"IF(E210 = CHAR(37), F210*G210/100,F210*G210)","v":{"v":0,"d":"0.00"}}]
[]
[25610,"3.1.12.2",null,"Floor and roof slabs","m²",{"v":21,"d":"21.00"},{"v":0,"d":"0.00"},{"$f":"IF(E212 = CHAR(37), F212*G212/100,F212*G212)","v":{"v":0,"d":"0.00"}}]
[]
[25611,"3.1.12.3",null,"Road crossing slab","m²",{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"$f":"IF(E214 = CHAR(37), F214*G214/100,F214*G214)","v":{"v":0,"d":"0.00"}}]
[]
[25548,"3.1.13","8.5","JOINTS"]
[]
[25549,"3.1.13.1",null,"Glassgrid to under asphalt at road crossing protection slab detail","m²",{"v":25,"d":"25.00"},{"v":0,"d":"0.00"},{"$f":"IF(E218 = CHAR(37), F218*G218/100,F218*G218)","v":{"v":0,"d":"0.00"}}]
[]
[25550,"3.1.13.2",null,"Concrete debonding agent to inner road crossing protection slab sides","m²",{"v":8,"d":"8.00"},{"v":0,"d":"0.00"},{"$f":"IF(E220 = CHAR(37), F220*G220/100,F220*G220)","v":{"v":0,"d":"0.00"}}]
[]
[25551,"3.1.13.3",null,"20mm polystyrene under road crossing protection slab","m²",{"v":7,"d":"7.00"},{"v":0,"d":"0.00"},{"$f":"IF(E222 = CHAR(37), F222*G222/100,F222*G222)","v":{"v":0,"d":"0.00"}}]
[]
[25559,null,null,"OFFTAKE CHAMBER DN500/400 PIPELINE OPTIONS ANALYSIS AND DESIGN"]
[]
[25560,"3.1.13.4","SANS 1200A 8.5(a)","Provide the provisional sum for the implementation of final agreed inlet works configuration including tie into existing raw water line, site run pipe, and other materials and works deemed necessary not included elsewhere within the BOQ to the screening structure.","Prov Sum",{"v":1,"d":"1.00"},{"v":750000,"d":"750,000.00"},{"v":750000,"d":"750,000.00"}]
[]
[25561,"3.1.13.5",null,"Contractors markup on the above direct proven costs","%",{"$f":"H226","v":{"v":750000,"d":"750,000.00"}},{"v":0,"d":"0.00"},{"$f":"IF(E228 = CHAR(37), F228*G228/100,F228*G228)","v":{"v":0,"d":"0.00"}}]
[]
[25562,"3.1.13.6",null,"Contractor to present options (inclusive of preliminary cost estimates) , workshop and finalise design including implementation methodology for the final agreed inlet works configuration. ","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E230 = CHAR(37), F230*G230/100,F230*G230)","v":{"v":0,"d":"0.00"}}]
[]
[25605,"3.1.14","SANS 1200L\r\nPSL","PIPE FITTINGS"]
{"$rows_empty":7}
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H201:H239)","v":{"v":750000,"d":"750,000.00"}}]
[null,"SCHEDULE 3 - HEAD OF WORKS"]
[{"$nulls":7},"SECTION 3: HEAD OF WORKS "]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H240","v":{"v":750000,"d":"750,000.00"}}]
[25563,null,null,"Supply deliver, install to site the following fittings to test and commission. All pressure rating PN10 and all Flange Drilling to match existing. Rates to include necessary couplings, sockets, flange jointing material, cutting, welding, joining, lining, coating, and coating repair on site as necessary.:"]
[]
[25564,"3.1.14.1",null,"Item 1, DN500, PN10 Epoxy coated and lined flanged restrained VJ coupling","No",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E247 = CHAR(37), F247*G247/100,F247*G247)","v":{"v":0,"d":"0.00"}}]
[]
[25565,"3.1.14.2",null,"Item 2, DN500, PN10 Epoxy coated and lined flanged pipe with puddle 1200mm long, 25mm stub, ball valve and pressure gauge","No",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E249 = CHAR(37), F249*G249/100,F249*G249)","v":{"v":0,"d":"0.00"}}]
[]
[25566,"3.1.14.3",null,"Item 4, DN500/400, PN10 Epoxy coated and lined flanged/plain ended concentric reducer 2300mm long","No",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E251 = CHAR(37), F251*G251/100,F251*G251)","v":{"v":0,"d":"0.00"}}]
[]
[25567,"3.1.14.4",null,"Item 5, DN400, PN10 Epoxy coated and lined flanged restrained VJ coupling","No",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E253 = CHAR(37), F253*G253/100,F253*G253)","v":{"v":0,"d":"0.00"}}]
[]
[25568,"3.1.14.5",null,"Item 7, DN400/500, PN10 Epoxy coated and lined flanged reducer special with puddle 1700mm long. ","No",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E255 = CHAR(37), F255*G255/100,F255*G255)","v":{"v":0,"d":"0.00"}}]
[]
[25569,"3.1.14.6",null,"Item 8, DN80, PN10 Epoxy coated GMS flanged/plain ended pipe with puddle 400mm long.","No",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E257 = CHAR(37), F257*G257/100,F257*G257)","v":{"v":0,"d":"0.00"}}]
[]
[25570,"3.1.14.7",null,"Item 9, DN80, PN10 Epoxy coated GMS flange adaptor for HDPe","No",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E259 = CHAR(37), F259*G259/100,F259*G259)","v":{"v":0,"d":"0.00"}}]
[]
[25571,"3.1.14.8",null,"DN500 Insulating flange as specified","No",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E261 = CHAR(37), F261*G261/100,F261*G261)","v":{"v":0,"d":"0.00"}}]
[]
[25572,"3.1.15","SANS 1200HA","SUNDRY ITEMS"]
[]
[25573,"3.1.15.1",null,"GMS access ladder fabricated to details on drawings and fixed to internal wall of chamber. Overall length 2.4m","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E265 = CHAR(37), F265*G265/100,F265*G265)","v":{"v":0,"d":"0.00"}}]
[]
[25574,"3.1.15.2",null,"GMS hand grip fabricated to detail on drawing and cast into slab","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E267 = CHAR(37), F267*G267/100,F267*G267)","v":{"v":0,"d":"0.00"}}]
[]
[25575,"3.1.15.3",null,"GMS pipe brackets for DN400 pipes as detailed","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E269 = CHAR(37), F269*G269/100,F269*G269)","v":{"v":0,"d":"0.00"}}]
[]
[25576,"3.1.15.4",null,"GMS pipe brackets for DN500 pipes as detailed","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E271 = CHAR(37), F271*G271/100,F271*G271)","v":{"v":0,"d":"0.00"}}]
[]
[25577,null,null,"GALVANISED/SS STEEL VENTILATORS"]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H244:H273)","v":{"v":750000,"d":"750,000.00"}}]
[null,"SCHEDULE 3 - HEAD OF WORKS"]
[{"$nulls":7},"SECTION 3: HEAD OF WORKS "]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H274","v":{"v":750000,"d":"750,000.00"}}]
[25578,"3.1.15.5",null,"Fabricate and install GMS ventilators to detail on drawings ","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E279 = CHAR(37), F279*G279/100,F279*G279)","v":{"v":0,"d":"0.00"}}]
[]
[25579,"3.1.16","SANS 1200HA","MISCELLANEOUS ITEMS"]
[]
[25580,null,null,"MANHOLE COVER "]
[]
[25581,"3.1.16.1",null,"Supply and install into roof of chambers 1.8x0.9m GMS lockable manhole cover and frame complete as detailed on the drawings ","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E285 = CHAR(37), F285*G285/100,F285*G285)","v":{"v":0,"d":"0.00"}}]
[]
[25582,"3.1.17","SANS 1200A","PROVISIONAL SUM"]
[]
[25583,"3.1.17.1","8.5(a)","Provide the Provisional Sum of R50 000 for  signage and life saving equipment as instructed by the Engineer","Prov Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E289 = CHAR(37), F289*G289/100,F289*G289)","v":{"v":0,"d":"0.00"}}]
[]
[25584,"3.1.17.2",null,"Contractors markup on above","%",{"$f":"H289","v":{"v":0,"d":"0.00"}},{"v":0,"d":"0.00"},{"$f":"IF(E291 = CHAR(37), F291*G291/100,F291*G291)","v":{"v":0,"d":"0.00"}}]
[]
[25585,null,null,"FLOW CONTROL VALVE CHAMBER AND SCREEN (Ref Drawing 60398/37) "]
[]
[25606,"3.1.18","SANS 1200D\r\nPSD","EARTHWORKS"]
[]
[25586,"3.1.18.1","8.3.1.2","Remove topsoil to a normal depth of 150mm stockpile & maintain","m²",{"v":90,"d":"90.00"},{"v":0,"d":"0.00"},{"$f":"IF(E297 = CHAR(37), F297*G297/100,F297*G297)","v":{"v":0,"d":"0.00"}}]
[]
[25587,"3.1.18.2","8.3.3","Restricted excavation in all materials irrespective of depth for chambers","m³",{"v":110,"d":"110.00"},{"v":0,"d":"0.00"},{"$f":"IF(E299 = CHAR(37), F299*G299/100,F299*G299)","v":{"v":0,"d":"0.00"}}]
[]
[25588,"3.1.18.3","8.3.6","Overhaul for spoil material under item 3.8.1.1/2 as instructed by the Engineer","m³.km",{"v":500,"d":"500.00"},{"v":0,"d":"0.00"},{"$f":"IF(E301 = CHAR(37), F301*G301/100,F301*G301)","v":{"v":0,"d":"0.00"}}]
[]
[25589,"3.1.19",null,"FINISHES"]
[]
[25590,"3.1.19.1","8.3.10","Topsoiling from stockpile under item 3.8.1.1","m²",{"v":60,"d":"60.00"},{"v":0,"d":"0.00"},{"$f":"IF(E305 = CHAR(37), F305*G305/100,F305*G305)","v":{"v":0,"d":"0.00"}}]
[]
[25591,"3.1.19.2","8.3.11","Supply and lay approved grassing as specified in the EMP","m²",{"v":60,"d":"60.00"},{"v":0,"d":"0.00"},{"$f":"IF(E307 = CHAR(37), F307*G307/100,F307*G307)","v":{"v":0,"d":"0.00"}}]
[]
[25592,null,"SANS 1200G\r\nPSG","CONCRETE WORKS (STRUCTURAL)"]
[]
[25593,"3.1.20","8.1.1","FORMWORK"]
[]
[25594,null,null,"Supply, install and remove upon completion all necessary formwork shutters, propping, scaffold support work, ledges, soldiers, keys, wedges and ferrels complete.  Rate inclusive of boxing out for pipework and manholes."]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H278:H314)","v":{"v":750000,"d":"750,000.00"}}]
[null,"SCHEDULE 3 - HEAD OF WORKS"]
[{"$nulls":7},"SECTION 3: HEAD OF WORKS "]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H315","v":{"v":750000,"d":"750,000.00"}}]
[25595,null,null,"Smooth vertical to chambers"]
[]
[25596,"3.1.20.1","8.2.2","Vertical wall surfaces to chambers","m²",{"v":85,"d":"85.00"},{"v":0,"d":"0.00"},{"$f":"IF(E322 = CHAR(37), F322*G322/100,F322*G322)","v":{"v":0,"d":"0.00"}}]
[]
[25597,null,null,"Narrow Widths to chambers not exceeding 250mm"]
[]
[25598,"3.1.20.2","8.2.5","External floor slab","m",{"v":26,"d":"26.00"},{"v":0,"d":"0.00"},{"$f":"IF(E326 = CHAR(37), F326*G326/100,F326*G326)","v":{"v":0,"d":"0.00"}}]
[]
[25599,"3.1.20.3","8.2.2","25 x 25mm extra over for chamfer to all exposed edges","m",{"v":60,"d":"60.00"},{"v":0,"d":"0.00"},{"$f":"IF(E328 = CHAR(37), F328*G328/100,F328*G328)","v":{"v":0,"d":"0.00"}}]
[]
[25600,null,null,"Smooth horizontal soffits to chambers including propped to:"]
[]
[25601,"3.1.20.4",null,"Soffit for roof slab 2.4m","m²",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E332 = CHAR(37), F332*G332/100,F332*G332)","v":{"v":0,"d":"0.00"}}]
[]
[25602,"3.1.21","8.1.2","REINFORCEMENT"]
[]
[25603,"3.1.21.1","8.3.1","High tensile steel reinforcement of all diameters between 8mm and 25mm in chamber floors, walls and roofs.","t",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E336 = CHAR(37), F336*G336/100,F336*G336)","v":{"v":0,"d":"0.00"}}]
[]
[25552,"3.1.21.2",null,"MS reinforcement of all diameters between 8mm and 32mm","t",{"v":0.1,"d":"0.10"},{"v":0,"d":"0.00"},{"$f":"IF(E338 = CHAR(37), F338*G338/100,F338*G338)","v":{"v":0,"d":"0.00"}}]
[]
[25553,"3.1.21.3","8.3.2","Mesh ref. 888","m²",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E340 = CHAR(37), F340*G340/100,F340*G340)","v":{"v":0,"d":"0.00"}}]
[]
[25554,"3.1.22","8.1.3","CONCRETE"]
[]
[25612,"3.1.22.1","PSG 5.5.3.2","Concrete mix designs","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E344 = CHAR(37), F344*G344/100,F344*G344)","v":{"v":0,"d":"0.00"}}]
[]
[25555,"3.1.22.2","8.4.2","Blinding layer 50mm thick in grade 15/19 concrete to chambers","m²",{"v":35,"d":"35.00"},{"v":0,"d":"0.00"},{"$f":"IF(E346 = CHAR(37), F346*G346/100,F346*G346)","v":{"v":0,"d":"0.00"}}]
[]
[25556,null,"8.4.3","Grade 30/19 concrete (min. cement content to be 350kg/m3) in chambers"]
[]
[25557,"3.1.22.3",null,"Chamber","m³",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E350 = CHAR(37), F350*G350/100,F350*G350)","v":{"v":0,"d":"0.00"}}]
[]
[25558,"3.1.22.4",null,"Screening Structure incl. skip slab","m³",{"v":18,"d":"18.00"},{"v":0,"d":"0.00"},{"$f":"IF(E352 = CHAR(37), F352*G352/100,F352*G352)","v":{"v":0,"d":"0.00"}}]
[]
[25381,"3.1.23",null,"UNFORMED SURFACE FINISHES"]
[]
[25382,null,"8.4.4 (b)","Steel float finish"]
[]
[25383,"3.1.23.1",null,"Chamber Floor Slabs","m²",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E358 = CHAR(37), F358*G358/100,F358*G358)","v":{"v":0,"d":"0.00"}}]
[]
[25384,"3.1.23.2",null,"Chamber Roof Slabs","m²",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"$f":"IF(E360 = CHAR(37), F360*G360/100,F360*G360)","v":{"v":0,"d":"0.00"}}]
[]
[25385,"3.1.23.3",null,"Screens Floor Slab","m²",{"v":20,"d":"20.00"},{"v":0,"d":"0.00"},{"$f":"IF(E362 = CHAR(37), F362*G362/100,F362*G362)","v":{"v":0,"d":"0.00"}}]
[]
[25386,"3.1.23.4",null,"150mm Thick Reinforced Skip Floor Slab","m²",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E364 = CHAR(37), F364*G364/100,F364*G364)","v":{"v":0,"d":"0.00"}}]
[]
[25613,"3.1.24","PSG 5.5.8\r\nPSG 8.4.7","CURING AND PROTECTION"]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H319:H367)","v":{"v":750000,"d":"750,000.00"}}]
[null,"SCHEDULE 3 - HEAD OF WORKS"]
[{"$nulls":7},"SECTION 3: HEAD OF WORKS "]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H368","v":{"v":750000,"d":"750,000.00"}}]
[25614,"3.1.24.1",null,"Walls and sides","m²",{"v":92,"d":"92.00"},{"v":0,"d":"0.00"},{"$f":"IF(E373 = CHAR(37), F373*G373/100,F373*G373)","v":{"v":0,"d":"0.00"}}]
[]
[25615,"3.1.24.2",null,"Floor and roof slabs","m²",{"v":26,"d":"26.00"},{"v":0,"d":"0.00"},{"$f":"IF(E375 = CHAR(37), F375*G375/100,F375*G375)","v":{"v":0,"d":"0.00"}}]
[]
[25616,"3.1.24.3",null,"Skip floor slab","m²",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E377 = CHAR(37), F377*G377/100,F377*G377)","v":{"v":0,"d":"0.00"}}]
[]
[25387,"3.1.25","SANS 1200L\r\nPSL","PIPE FITTING"]
[]
[25388,null,null,"Supply deliver, install, test and commission the following items. Rates to include necessary couplings, sockets, flange jointing material, cutting, welding, joining, lining, coating, and coating repair on site as necessary.:"]
[]
[25389,"3.1.25.1",null,"Item 1, DN500 PN10 Epoxy coated and lined flanged/plain ended pipe 1170mm long with puddle.","No",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E383 = CHAR(37), F383*G383/100,F383*G383)","v":{"v":0,"d":"0.00"}}]
[]
[25390,"3.1.25.2",null,"Item 3,DN500 PN10 Epoxy coated and lined flanged VJ coupling.","No",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E385 = CHAR(37), F385*G385/100,F385*G385)","v":{"v":0,"d":"0.00"}}]
[]
[25391,"3.1.25.3",null,"Item 4\r\n, DN500 PN10 Epoxy coated and lined plain ended pipe 755mm long with puddle.","No",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E387 = CHAR(37), F387*G387/100,F387*G387)","v":{"v":0,"d":"0.00"}}]
[]
[25392,"3.1.25.4",null,"Item 5, DN400 PN10 Epoxy coated and lined plain ended pipe 755mm long with puddle.(1No. for bypass installation to exist. Mixing structure)","No",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E389 = CHAR(37), F389*G389/100,F389*G389)","v":{"v":0,"d":"0.00"}}]
[]
[25393,"3.1.25.5",null,"Item 6, DN500 PN10 Epoxy coated and lined plain ended pipe 550mm long with puddle.","No",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E391 = CHAR(37), F391*G391/100,F391*G391)","v":{"v":0,"d":"0.00"}}]
[]
[25394,"3.1.25.6",null,"Item 7, DN100 PN10 GMS and epoxy coated flanged/plain ended pipe welded to DN400 bypass pipeline 380mm long.","No",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E393 = CHAR(37), F393*G393/100,F393*G393)","v":{"v":0,"d":"0.00"}}]
[]
[25395,"3.1.25.7",null,"Item 8, DN100 PN10 GMS and epoxy coated flanged spool pipe 500mm long with puddle. ","No",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E395 = CHAR(37), F395*G395/100,F395*G395)","v":{"v":0,"d":"0.00"}}]
[]
[25396,"3.1.25.8",null,"Item 9, DN100 PN10 GMS and epoxy coated flanged/plain ended pipe 980mm long. ","No",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E397 = CHAR(37), F397*G397/100,F397*G397)","v":{"v":0,"d":"0.00"}}]
[]
[25397,"3.1.25.9",null,"Item 10, DN100 PN10 epoxy coated and lined VJ coupling.","No",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E399 = CHAR(37), F399*G399/100,F399*G399)","v":{"v":0,"d":"0.00"}}]
[]
[25398,"3.1.25.10",null,"Item 11, DN100 PN10 epoxy coated and lined SGI resilient seal gate valve.","No",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E401 = CHAR(37), F401*G401/100,F401*G401)","v":{"v":0,"d":"0.00"}}]
[]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H372:H403)","v":{"v":750000,"d":"750,000.00"}}]
[null,"SCHEDULE 3 - HEAD OF WORKS"]
[{"$nulls":7},"SECTION 3: HEAD OF WORKS "]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H404","v":{"v":750000,"d":"750,000.00"}}]
[25399,"3.1.25.11",null,"Item 12, DN100 PN10 GMS and epoxy coated flanged 90° LR bend special with puddle 630mm long","No",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E409 = CHAR(37), F409*G409/100,F409*G409)","v":{"v":0,"d":"0.00"}}]
[]
[25400,"3.1.25.12",null,"Item 13, DN100 PN10 GMS and epoxy coated flanged spool pipe 3860mm long. ","No",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E411 = CHAR(37), F411*G411/100,F411*G411)","v":{"v":0,"d":"0.00"}}]
[]
[25401,"3.1.25.13",null,"Item 14, DN100 PN10 GMS and epoxy coated flanged/plain ended 90° LR bend special with puddle 365mm long","No",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E413 = CHAR(37), F413*G413/100,F413*G413)","v":{"v":0,"d":"0.00"}}]
[]
[25402,"3.1.25.14",null,"Item 15, DN80 PN10 Epoxy coated GMS flanged one end spool pipe with puddle 400mm long","No",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E415 = CHAR(37), F415*G415/100,F415*G415)","v":{"v":0,"d":"0.00"}}]
[]
[25403,"3.1.25.15",null,"Item 16, DN80 PN10 Epoxy coated and lined flange adaptor for HDPE.","No",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E417 = CHAR(37), F417*G417/100,F417*G417)","v":{"v":0,"d":"0.00"}}]
[]
[25404,"3.1.25.16",null,"DN75 HDPe pipe site run to daylight","m",{"v":15,"d":"15.00"},{"v":0,"d":"0.00"},{"$f":"IF(E419 = CHAR(37), F419*G419/100,F419*G419)","v":{"v":0,"d":"0.00"}}]
[]
[25405,"3.1.25.17",null,"DN500 D75 concrete pipeline site run to headwall","m",{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"$f":"IF(E421 = CHAR(37), F421*G421/100,F421*G421)","v":{"v":0,"d":"0.00"}}]
[]
[25406,"3.1.26","SANS 1200HA","SUNDRY ITEMS"]
[]
[25407,"3.1.26.1",null,"GRP access ladder fabricated to details on drawings and fixed to internal wall of chamber. Overall length 2.4m","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E425 = CHAR(37), F425*G425/100,F425*G425)","v":{"v":0,"d":"0.00"}}]
[]
[25408,"3.1.26.2","8.3.2 (b)","Supply, fabricate, deliver and install coated GMS ball type handrailing, Height & style to match existing. (including sloped as shown), complete.","m",{"v":30,"d":"30.00"},{"v":0,"d":"0.00"},{"$f":"IF(E427 = CHAR(37), F427*G427/100,F427*G427)","v":{"v":0,"d":"0.00"}}]
[]
[25409,"3.1.26.3",null,"Swing gate to ball type handrailing as detailed ","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E429 = CHAR(37), F429*G429/100,F429*G429)","v":{"v":0,"d":"0.00"}}]
[]
[25410,"3.1.26.4",null,"GMS pipe brackets for DN500 pipes as detailed","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E431 = CHAR(37), F431*G431/100,F431*G431)","v":{"v":0,"d":"0.00"}}]
[]
[25411,"3.1.26.5",null,"Supply, fabricate, deliver and install 40x40 GMS grating (40x3 bearer bar). Grating segments to be banded. Holes to manufactured for items such as hand railing stanchions, hand stop slits.","m²",{"v":3.5,"d":"3.50"},{"v":0,"d":"0.00"},{"$f":"IF(E433 = CHAR(37), F433*G433/100,F433*G433)","v":{"v":0,"d":"0.00"}}]
[]
[25412,"3.1.26.6",null,"Supply, fabricate, deliver and install 50x50(x5mm) GMS support beam for grating, fixed to wall with galv. M12 chemical anchors at 300mm spacing","m",{"v":2.5,"d":"2.50"},{"v":0,"d":"0.00"},{"$f":"IF(E435 = CHAR(37), F435*G435/100,F435*G435)","v":{"v":0,"d":"0.00"}}]
[]
[]
[]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H408:H439)","v":{"v":750000,"d":"750,000.00"}}]
[null,"SCHEDULE 3 - HEAD OF WORKS"]
[{"$nulls":7},"SECTION 3: HEAD OF WORKS "]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H440","v":{"v":750000,"d":"750,000.00"}}]
[25413,"3.1.26.7",null,"Supply, fabricate, deliver and cast in 40x40(x3mm) GMS support bracket for grating, cast in with fishtails at 300mm centres.","m",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E445 = CHAR(37), F445*G445/100,F445*G445)","v":{"v":0,"d":"0.00"}}]
[]
[25414,"3.1.26.8",null,"Galv. Skip skid 40kg/m rail steel section cast into proposed slab 2.5m long","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E447 = CHAR(37), F447*G447/100,F447*G447)","v":{"v":0,"d":"0.00"}}]
[]
[25415,"3.1.27","SANS 1200G\r\nPSG","JOINTS"]
[]
[25416,"3.1.27.1","8.5","200 x 2mm thick sikadur combiflex system or similar approved ","m",{"v":25,"d":"25.00"},{"v":0,"d":"0.00"},{"$f":"IF(E451 = CHAR(37), F451*G451/100,F451*G451)","v":{"v":0,"d":"0.00"}}]
[]
[25417,"3.1.27.2","8.5","250 x 3mm thick plasticized PVC type control waterbar with clips to reinforcing ","m",{"v":25,"d":"25.00"},{"v":0,"d":"0.00"},{"$f":"IF(E453 = CHAR(37), F453*G453/100,F453*G453)","v":{"v":0,"d":"0.00"}}]
[]
[25418,"3.1.27.3","8.5","\"Sikaswell P\" Extrudable Water swelling Profile joint sealing waterstop (Provisional)","m",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E455 = CHAR(37), F455*G455/100,F455*G455)","v":{"v":0,"d":"0.00"}}]
[]
[25419,"3.1.28",null,"FIRE SAFETY"]
[]
[25420,"3.1.28.1",null,"Supply and install 5kg DCP fire extinguisher to wall, complete with weather cabinet and signage.","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E459 = CHAR(37), F459*G459/100,F459*G459)","v":{"v":0,"d":"0.00"}}]
[]
[25421,"3.1.28.2",null,"Supply and install 5kg CO2 fire extinguisher to wall, complete with weather cabinet and signage.","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E461 = CHAR(37), F461*G461/100,F461*G461)","v":{"v":0,"d":"0.00"}}]
[]
[25422,"3.1.29",null,"TESTING AND COMMISSIONING "]
[]
[25423,"3.1.29.1","PSG 7.3.9","Testing of screening structure for water tightness in accordance with the specifications.","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E465 = CHAR(37), F465*G465/100,F465*G465)","v":{"v":0,"d":"0.00"}}]
[]
[25424,"3.1.30",null,"GALVANISED/SS STEEL VENTILATORS"]
[]
[25425,"3.1.30.1",null,"Fabricate and install GMS ventilators to detail on drawings ","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E469 = CHAR(37), F469*G469/100,F469*G469)","v":{"v":0,"d":"0.00"}}]
[]
[25426,"3.1.31","SANS 1200HA","MISCELLANEOUS ITEMS"]
[]
[25427,"3.1.31.1",null,"Supply and install into roof of chambers 1.4x0.9m GMS lockable manhole cover and frame complete as detailed on the drawings ","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E473 = CHAR(37), F473*G473/100,F473*G473)","v":{"v":0,"d":"0.00"}}]
[]
[25428,"3.1.31.2",null,"0.5 Tonne screen and handstop hoist as detailed","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E475 = CHAR(37), F475*G475/100,F475*G475)","v":{"v":0,"d":"0.00"}}]
[]
[]
[]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H444:H479)","v":{"v":750000,"d":"750,000.00"}}]
[null,"SCHEDULE 3 - HEAD OF WORKS"]
[{"$nulls":7},"SECTION 3: HEAD OF WORKS "]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H480","v":{"v":750000,"d":"750,000.00"}}]
[25429,"3.1.31.3",null,"Provisional sum of R60000 for procurement of a Refuse Skip 3.5m³ or maintenance contract, period unspecified","Prov Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E485 = CHAR(37), F485*G485/100,F485*G485)","v":{"v":0,"d":"0.00"}}]
[]
[25430,"3.1.31.4",null,"Contractors markup on above","%",{"$f":"H485","v":{"v":0,"d":"0.00"}},{"v":0,"d":"0.00"},{"$f":"IF(E487 = CHAR(37), F487*G487/100,F487*G487)","v":{"v":0,"d":"0.00"}}]
[]
[25431,"3.1.32","SANS 1200A","PROVISIONAL SUM"]
[]
[25432,"3.1.32.1","8.5 (a)","Provide the Provisional Sum of R25 000 for chamber signage and painting as instructed by the Engineer","Prov Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E491 = CHAR(37), F491*G491/100,F491*G491)","v":{"v":0,"d":"0.00"}}]
[]
[25433,"3.1.32.2",null,"Contractors markup on above","%",{"$f":"H491","v":{"v":0,"d":"0.00"}},{"v":0,"d":"0.00"},{"$f":"IF(E493 = CHAR(37), F493*G493/100,F493*G493)","v":{"v":0,"d":"0.00"}}]
[]
[25434,"3.1.33",null,"POLYMER TANK BUND (Ref Drawing 60398/41)"]
[]
[25435,"3.1.33.1",null,"Clean out existing tanks and remove grating and other fixtures to stores / landfill as instructed.","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E497 = CHAR(37), F497*G497/100,F497*G497)","v":{"v":0,"d":"0.00"}}]
[]
[25436,"3.1.33.2",null,"Commercial bedding Sand fill compacted to 100% MOD AASHTO to existing polymer tank to required level.","m³",{"v":20,"d":"20.00"},{"v":0,"d":"0.00"},{"$f":"IF(E499 = CHAR(37), F499*G499/100,F499*G499)","v":{"v":0,"d":"0.00"}}]
[]
[25437,"3.1.34","SANS 1200G\r\nPSG","CONCRETE WORKS"]
[]
[25438,"3.1.34.1","8.5","Prepare Construction Joint (to new bund floor / wall interface) by removing outer concrete laitance (through needle punching or other approved method) and wetting for 24 hours before placing new concrete.","m²",{"v":6,"d":"6.00"},{"v":0,"d":"0.00"},{"$f":"IF(E503 = CHAR(37), F503*G503/100,F503*G503)","v":{"v":0,"d":"0.00"}}]
[]
[25439,"3.1.35","8.1.1","FORMWORK"]
[]
[25440,"3.1.35.1","8.2.5","Smooth vertical  to sump sides (125mm)","m",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E507 = CHAR(37), F507*G507/100,F507*G507)","v":{"v":0,"d":"0.00"}}]
[]
[25441,"3.1.35.2",null,"Supply and lay 250 micron plastic sheeting to underside of new concrete slab","m²",{"v":13,"d":"13.00"},{"v":0,"d":"0.00"},{"$f":"IF(E509 = CHAR(37), F509*G509/100,F509*G509)","v":{"v":0,"d":"0.00"}}]
[]
[25442,"3.1.36","8.1.2","REINFORCING"]
[]
[25443,"3.1.36.1",null,"Drill horizontal 150mm into existing tank walls and anchor (using anchoring adhesive) for Y12 dowel bars (priced below as part of reinforcing).","No.",{"v":200,"d":"200.00"},{"v":0,"d":"0.00"},{"$f":"IF(E513 = CHAR(37), F513*G513/100,F513*G513)","v":{"v":0,"d":"0.00"}}]
[]
[25444,"3.1.36.2","8.3.1","High tensile Reinforcing bars up to 32mm dia.","t",{"v":0.9,"d":"0.90"},{"v":0,"d":"0.00"},{"$f":"IF(E515 = CHAR(37), F515*G515/100,F515*G515)","v":{"v":0,"d":"0.00"}}]
[]
[25445,"3.1.36.3","8.3.2","Mesh ref 888","m²",{"v":27,"d":"27.00"},{"v":0,"d":"0.00"},{"$f":"IF(E517 = CHAR(37), F517*G517/100,F517*G517)","v":{"v":0,"d":"0.00"}}]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H484:H518)","v":{"v":750000,"d":"750,000.00"}}]
[null,"SCHEDULE 3 - HEAD OF WORKS"]
[{"$nulls":7},"SECTION 3: HEAD OF WORKS "]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H519","v":{"v":750000,"d":"750,000.00"}}]
[25446,"3.1.37","8.1.3","CONCRETE"]
[]
[25447,"3.1.37.1","PSG 5.5.3.2","Concrete mix design","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E526 = CHAR(37), F526*G526/100,F526*G526)","v":{"v":0,"d":"0.00"}}]
[]
[25617,"3.1.37.2","8.4.3","25MPa/19mm concrete to bund floor & sump","m³",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"$f":"IF(E528 = CHAR(37), F528*G528/100,F528*G528)","v":{"v":0,"d":"0.00"}}]
[]
[25448,"3.1.37.3","8.5","Grind out 25mm wide by 20mm deep around perimeter joint, prime, and fill with Xypex concentrate or similar approved crystalline waterproofing grout mixture.","m",{"v":21,"d":"21.00"},{"v":0,"d":"0.00"},{"$f":"IF(E530 = CHAR(37), F530*G530/100,F530*G530)","v":{"v":0,"d":"0.00"}}]
[]
[25449,"3.1.38",null,"UNFORMED SURFACE FINISHES"]
[]
[25450,"3.1.38.1","8.4.4 (b)","Steel-floated finish to top of bund slab and sump.","m²",{"v":14,"d":"14.00"},{"v":0,"d":"0.00"},{"$f":"IF(E534 = CHAR(37), F534*G534/100,F534*G534)","v":{"v":0,"d":"0.00"}}]
[]
[25618,"3.1.39","PSG 5.5.8\r\nPSG 8.4.7","CURING AND PROTECTION"]
[]
[25619,"3.1.39.1",null,"Bund slab and sump","m²",{"v":14,"d":"14.00"},{"v":0,"d":"0.00"},{"$f":"IF(E538 = CHAR(37), F538*G538/100,F538*G538)","v":{"v":0,"d":"0.00"}}]
[]
[25451,"3.1.40","SANS 1200HA","STRUCTURAL STEELWORK"]
[]
[25452,null,null,"Rates to include installation and corrosion protection as specified."]
[]
[25453,"3.1.40.1","8.3.3","Supply and install GMS ladders as detailed, complete with top extension hand grip as shown and cross bracing for hanging ladder.","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E544 = CHAR(37), F544*G544/100,F544*G544)","v":{"v":0,"d":"0.00"}}]
[]
[25454,"3.1.40.2","8.3.3","Supply and install GMS ladders as detailed into bund sump.","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E546 = CHAR(37), F546*G546/100,F546*G546)","v":{"v":0,"d":"0.00"}}]
[]
[25455,"3.1.40.3","8.3.4","Supply, fabricate, deliver and install 40x40 GMS grating (RS40 40x4.5). Grating segments to be banded.","m²",{"v":12.5,"d":"12.50"},{"v":0,"d":"0.00"},{"$f":"IF(E548 = CHAR(37), F548*G548/100,F548*G548)","v":{"v":0,"d":"0.00"}}]
[]
[25456,"3.1.40.4",null,"Extra over above to form 700 (600 internal) opening for removable grating manhole.","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E550 = CHAR(37), F550*G550/100,F550*G550)","v":{"v":0,"d":"0.00"}}]
[]
[25457,"3.1.40.5",null,"700mm removable grating manhole fitted into GMS grating stated above.","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E552 = CHAR(37), F552*G552/100,F552*G552)","v":{"v":0,"d":"0.00"}}]
[]
[25458,"3.1.40.6","8.3.2 (b)","Supply, fabricate, deliver and install coated GMS ball type handrailing to bund wall, to tie into existing. Height & style to match existing.","m",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E554 = CHAR(37), F554*G554/100,F554*G554)","v":{"v":0,"d":"0.00"}}]
[]
[25459,"3.1.40.7",null,"Safety chain to 1t breaking load to the above hand railing","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E556 = CHAR(37), F556*G556/100,F556*G556)","v":{"v":0,"d":"0.00"}}]
[]
[25460,"3.1.40.8","8.3.1","Galv. IPE200 S355 installed to grating support, fixed at ends.","m",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E558 = CHAR(37), F558*G558/100,F558*G558)","v":{"v":0,"d":"0.00"}}]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H523:H559)","v":{"v":750000,"d":"750,000.00"}}]
[null,"SCHEDULE 3 - HEAD OF WORKS"]
[{"$nulls":7},"SECTION 3: HEAD OF WORKS "]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H560","v":{"v":750000,"d":"750,000.00"}}]
[25461,"3.1.40.9","8.3.1","Galv. 100x100x8mm S355 angle section to walls for grating support, with galv. M12 chemical anchors (150mm deep) spaced at 300 centres,","m",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E565 = CHAR(37), F565*G565/100,F565*G565)","v":{"v":0,"d":"0.00"}}]
[]
[25462,"3.1.40.10",null,"350mm DN50 HDPe pipe to sump drain, cored and cast into wall with Xypex concentrate mix (or similar approved) with ball valve. ","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E567 = CHAR(37), F567*G567/100,F567*G567)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":49}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H564:H616)","v":{"v":750000,"d":"750,000.00"}}]
[null,"SCHEDULE 3 - HEAD OF WORKS"]
[{"$nulls":3},"SUMMARY OF SECTIONS"]
[null," ","SECTION","DESCRIPTION",{"$nulls":3},"AMOUNT\n(RAND)"]
[null,null,"3.1","SECTION 3: HEAD OF WORKS ",{"$nulls":3},{"$f":"H617","v":{"v":750000,"d":"750,000.00"}}]
{"$rows_empty":57}
[null,null," Total Carried Forward To Summary Of Schedules"," Total Carried Forward To Summary Of Schedules",{"$nulls":3},{"$f":"SUM(H621:H678)","v":{"v":750000,"d":"750,000.00"}}]

{"sheet":"Schedule 4","index":3,"n_rows":488,"n_cols":8,"rows_kept":488}
["Rate=G","SCHEDULE 4 - FLOCCULATION TANKS"]
[{"$nulls":7},"SECTION 4: FLOCCULATION TANKS"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[25127,"4.1",null,"SECTION 4: FLOCCULATION TANKS"]
[]
[25128,"4.1.1","SANS 1200C\r\nPSC","SITE CLEARANCE "]
[]
[25129,"4.1.1.1","8.2.1","Clear and grub site","m²",{"v":300,"d":"300.00"},{"v":0,"d":"0.00"},{"$f":"IF(E8 = CHAR(37), F8*G8/100,F8*G8)","v":{"v":0,"d":"0.00"}}]
[]
[25130,"4.1.1.2","8.2.8","Demolition of existing inlet works to limit of demolition as shown, including removal from site to registered land fill. Demolition to only commence when new inlet works with temporary bypass line has been completed (including dosing and mechanicals etc. complete) and water redirected. ","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E10 = CHAR(37), F10*G10/100,F10*G10)","v":{"v":0,"d":"0.00"}}]
[]
[25131,"4.1.2","SANS 1200 D\r\nPSD","EARTHWORKS"]
[]
[25132,"4.1.2.1","8.3.1.2","Remove topsoil to a normal depth of 150mm stockpile & maintain in accordance with the environmental specifications. ","m²",{"v":300,"d":"300.00"},{"v":0,"d":"0.00"},{"$f":"IF(E14 = CHAR(37), F14*G14/100,F14*G14)","v":{"v":0,"d":"0.00"}}]
[]
[25133,"4.1.3","8.3.3","RESTRICTED EXCAVATION"]
[]
[25134,"4.1.3.1","8.3.3","Restricted excavation in all materials and use for embankment or backfill or dispose, as ordered (freehaul of 1.0km)","m³",{"v":600,"d":"600.00"},{"v":0,"d":"0.00"},{"$f":"IF(E18 = CHAR(37), F18*G18/100,F18*G18)","v":{"v":0,"d":"0.00"}}]
[]
[25135,null,"8.3.3.2","Extra-over items 4.3.1 for in:"]
[]
[25136,"4.1.3.2",null,"2) Hard Rock excavation ","m³",{"v":30,"d":"30.00"},{"v":0,"d":"0.00"},{"$f":"IF(E22 = CHAR(37), F22*G22/100,F22*G22)","v":{"v":0,"d":"0.00"}}]
[]
[25137,"4.1.4","8.3.4","IMPORTED MATERIAL"]
[]
[25138,"4.1.4.1",null,"a) One layer 150mm G5 from commercial source compacted to 93% mod Aashto under blinding.","m³",{"v":30,"d":"30.00"},{"v":0,"d":"0.00"},{"$f":"IF(E26 = CHAR(37), F26*G26/100,F26*G26)","v":{"v":0,"d":"0.00"}}]
[]
[25139,"4.1.5","8.3.6","OVERHAUL"]
[]
[25140,"4.1.5.1",null,"b) Long Overhaul (provisional) for material to spoil","m³.km",{"v":1200,"d":"1,200.00"},{"v":0,"d":"0.00"},{"$f":"IF(E30 = CHAR(37), F30*G30/100,F30*G30)","v":{"v":0,"d":"0.00"}}]
[]
[25141,"4.1.6",null,"FINISHING "]
[]
[25142,"4.1.6.1","8.3.10","Top soiling 150mm thick from stock pile item above.","m²",{"v":140,"d":"140.00"},{"v":0,"d":"0.00"},{"$f":"IF(E34 = CHAR(37), F34*G34/100,F34*G34)","v":{"v":0,"d":"0.00"}}]
[]
[25143,"4.1.6.2","8.3.11","Grassing as specified in the environmental specifications.","m²",{"v":140,"d":"140.00"},{"v":0,"d":"0.00"},{"$f":"IF(E36 = CHAR(37), F36*G36/100,F36*G36)","v":{"v":0,"d":"0.00"}}]
[]
[25144,"4.1.7","SANS 1200F"," PILING"]
[]
[]
[]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H4:H42)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 4 - FLOCCULATION TANKS"]
[{"$nulls":7},"SECTION 4: FLOCCULATION TANKS"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H43","v":{"v":0,"d":"0.00"}}]
[25145,null,null,"End-bearing auger/bore replacement type piling designed by specialist piling (550 kN max load, 150kN max. tension load) contractor including minimum 3 x Diameter rock socket, freehaul of 1.0km, reinforcing, concrete, etc. complete. The pile design should allow for 55kN horizontal load and top connection moment of 100kN.m. To be designed for severe exposure conditions and 50 year life span.  To be submitted for approval."]
[]
[25146,"4.1.7.1","8.2.1","Establishment on Site for Piling","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E50 = CHAR(37), F50*G50/100,F50*G50)","v":{"v":0,"d":"0.00"}}]
[]
[25147,"4.1.7.2","8.2.2","Move Equipment to and set up at each Pile Position","No.",{"v":18,"d":"18.00"},{"v":0,"d":"0.00"},{"$f":"IF(E52 = CHAR(37), F52*G52/100,F52*G52)","v":{"v":0,"d":"0.00"}}]
[]
[25148,null,null,"Piling though material situated in the following successive depth ranges. Including auguring/boring through obstructions, temporary casings, reinforcing, concrete, stripping/cutting pile head, etc complete as deemed required."]
[]
[25149,"4.1.7.3",null,"a) over 0m and up to 10m","m",{"v":180,"d":"180.00"},{"v":0,"d":"0.00"},{"$f":"IF(E56 = CHAR(37), F56*G56/100,F56*G56)","v":{"v":0,"d":"0.00"}}]
[]
[25150,"4.1.7.4",null,"b) over 10m and up to 15m","m",{"v":27,"d":"27.00"},{"v":0,"d":"0.00"},{"$f":"IF(E58 = CHAR(37), F58*G58/100,F58*G58)","v":{"v":0,"d":"0.00"}}]
[]
[25151,"4.1.7.5",null,"c) over 15m and up to 20m","m",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E60 = CHAR(37), F60*G60/100,F60*G60)","v":{"v":0,"d":"0.00"}}]
[]
[25152,"4.1.7.6",null,"Low energy Frequency Response dynamic pile integrity testing on all piles by independent specialist consultant.","No.",{"v":18,"d":"18.00"},{"v":0,"d":"0.00"},{"$f":"IF(E62 = CHAR(37), F62*G62/100,F62*G62)","v":{"v":0,"d":"0.00"}}]
[]
[25153,"4.1.7.7",null,"Installation of (complete), and Load testing of additional piles to destruction (Dynamic Load Test)","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E64 = CHAR(37), F64*G64/100,F64*G64)","v":{"v":0,"d":"0.00"}}]
[]
[25154,"4.1.8","SANS 1200G\r\nPSG","CONCRETE (STRUCTURAL)"]
[]
[25257,null,null,"SUPPLEMENTARY PREAMBLES:"]
[]
[25258,null,null,"Cost of tests"]
{"$rows_empty":10}
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H47:H80)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 4 - FLOCCULATION TANKS"]
[{"$nulls":7},"SECTION 4: FLOCCULATION TANKS"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H81","v":{"v":0,"d":"0.00"}}]
[25259,null,null,"The costs of making, storing and testing of concrete test cubes as required under clause 7 \"Tests\" of SANS 1200 G shall include the cost of providing cube moulds necessary for the purpose, for testing costs and for submitting reports on the tests to the Engineer. The testing shall be undertaken by an independent firm or institution nominated by the contractor to the approval of the Engineer. (Number of test to be included in accordance with SANS1200G)"]
[]
[25260,null,null,"Formwork"]
[]
[25261,null,null,"Descriptions of formwork shall be deemed to include use and waste only (except where described as \"left in\" or \"permanent\"), for fitting together in the required forms, wedging, plumbing and fixing to true angles and surfaces as necessary to ensure easy release during stripping and for reconditioning as necessary before re-use"]
[]
[25262,null,null,"The vertical strutting shall be carried down to such construction as is sufficiently strong to afford the required support without damage and shall remain in position until the newly constructed work is able to support itself"]
[]
[25263,null,null,"Formwork to soffits of solid slabs etc shall be deemed to be to slabs not exceeding 250mm thick unless otherwise described"]
[]
[25264,null,null,"Formwork to soffits of slabs, beams, etc shall be deemed to be propped up exceeding 1,5m and not exceeding 3,5m high unless otherwise described"]
[]
[25265,null,null,"Formwork to sides of bases, ground beams, etc will only be measured where it is prescribed by the engineer for design reasons. Formwork necessitated by irregularity or collapse of excavated faces will not be measured and the cost thereof shall be deemed to be included in the allowance for taking the risk of collapse of the sides of the excavations, provision for which is made in \"Earthworks\""]
[]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H85:H100)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 4 - FLOCCULATION TANKS"]
[{"$nulls":7},"SECTION 4: FLOCCULATION TANKS"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H101","v":{"v":0,"d":"0.00"}}]
[25155,"4.1.9","8.1.1\r\nPSG8.2.2","FORMWORK"]
[]
[25156,null,null,"Vertical formwork"]
[]
[25157,"4.1.9.1",null,"Screed/plaster vertical sides to pile caps (to serve as external pile cap permanent shutter.","m²",{"v":30,"d":"30.00"},{"v":0,"d":"0.00"},{"$f":"IF(E110 = CHAR(37), F110*G110/100,F110*G110)","v":{"v":0,"d":"0.00"}}]
[]
[25158,"4.1.9.2","8.2.1","Rough vertical to Sides of flocculation tank base","m²",{"v":16,"d":"16.00"},{"v":0,"d":"0.00"},{"$f":"IF(E112 = CHAR(37), F112*G112/100,F112*G112)","v":{"v":0,"d":"0.00"}}]
[]
[25159,"4.1.9.3","8.2.2","Smooth vertical to Flocculation tank","m²",{"v":280,"d":"280.00"},{"v":0,"d":"0.00"},{"$f":"IF(E114 = CHAR(37), F114*G114/100,F114*G114)","v":{"v":0,"d":"0.00"}}]
[]
[25160,"4.1.9.4","8.2.2","Smooth vertical to Inlet channel and chamber ","m²",{"v":120,"d":"120.00"},{"v":0,"d":"0.00"},{"$f":"IF(E116 = CHAR(37), F116*G116/100,F116*G116)","v":{"v":0,"d":"0.00"}}]
[]
[25161,"4.1.9.5","8.2.2","Smooth vertical to baffle walls (rapid mix inlet channel)","m²",{"v":12,"d":"12.00"},{"v":0,"d":"0.00"},{"$f":"IF(E118 = CHAR(37), F118*G118/100,F118*G118)","v":{"v":0,"d":"0.00"}}]
[]
[25162,"4.1.9.6","8.2.2","Smooth vertical to Outlet channel","m²",{"v":32,"d":"32.00"},{"v":0,"d":"0.00"},{"$f":"IF(E120 = CHAR(37), F120*G120/100,F120*G120)","v":{"v":0,"d":"0.00"}}]
[]
[25163,"4.1.9.7","8.2.2","Smooth vertical (including curved) to connecting channel","m²",{"v":43,"d":"43.00"},{"v":0,"d":"0.00"},{"$f":"IF(E122 = CHAR(37), F122*G122/100,F122*G122)","v":{"v":0,"d":"0.00"}}]
[]
[25164,"4.1.9.8","8.2.2","Smooth vertical to stairs","m²",{"v":3,"d":"3.00"},{"v":0,"d":"0.00"},{"$f":"IF(E124 = CHAR(37), F124*G124/100,F124*G124)","v":{"v":0,"d":"0.00"}}]
[]
[25165,"4.1.9.9",null,"Formwork for steps","No",{"v":12,"d":"12.00"},{"v":0,"d":"0.00"},{"$f":"IF(E126 = CHAR(37), F126*G126/100,F126*G126)","v":{"v":0,"d":"0.00"}}]
[]
[25166,null,null,"Horizontal formwork"]
[]
[25167,"4.1.9.10","8.2.2","Smooth horizontal to walkway slabs","m²",{"v":38,"d":"38.00"},{"v":0,"d":"0.00"},{"$f":"IF(E130 = CHAR(37), F130*G130/100,F130*G130)","v":{"v":0,"d":"0.00"}}]
[]
[25168,null,null,"Narrow widths"]
[]
[25169,"4.1.9.11","8.2.5","150mm Smooth horizontal narrow to walkway sides","m",{"v":53,"d":"53.00"},{"v":0,"d":"0.00"},{"$f":"IF(E134 = CHAR(37), F134*G134/100,F134*G134)","v":{"v":0,"d":"0.00"}}]
[]
[25170,"4.1.9.12","8.2.5","250mm Smooth horizontal narrow to underside of walls (inlet chamber, inlet channel, and central wall openings)","m",{"v":12,"d":"12.00"},{"v":0,"d":"0.00"},{"$f":"IF(E136 = CHAR(37), F136*G136/100,F136*G136)","v":{"v":0,"d":"0.00"}}]
[]
[25171,"4.1.9.13","8.2.5","250x250 vertical smooth column shutter to central wall column, flocculation tanks","m",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E138 = CHAR(37), F138*G138/100,F138*G138)","v":{"v":0,"d":"0.00"}}]
[]
[25172,"4.1.9.14","8.2.5","250mm smooth vertical narrow widths to wall openings (sides of weirs, outlets, and central wall bottom holes)","m",{"v":20,"d":"20.00"},{"v":0,"d":"0.00"},{"$f":"IF(E140 = CHAR(37), F140*G140/100,F140*G140)","v":{"v":0,"d":"0.00"}}]
[]
[25173,null,null,"Box-outs / form voids"]
[]
[25174,"4.1.9.15","8.2.6 (b)","Form voids in walkway slab for mixers, 300 dia.","No.",{"v":8,"d":"8.00"},{"v":0,"d":"0.00"},{"$f":"IF(E144 = CHAR(37), F144*G144/100,F144*G144)","v":{"v":0,"d":"0.00"}}]
[]
[25175,"4.1.9.16",null,"50mm PVC pipes cast into baffle walls","No.",{"v":35,"d":"35.00"},{"v":0,"d":"0.00"},{"$f":"IF(E146 = CHAR(37), F146*G146/100,F146*G146)","v":{"v":0,"d":"0.00"}}]
[]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H105:H148)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 4 - FLOCCULATION TANKS"]
[{"$nulls":7},"SECTION 4: FLOCCULATION TANKS"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H149","v":{"v":0,"d":"0.00"}}]
[25176,"4.1.9.17","8.2.6 (d)","Other than circular, up to and including 0.1m² up to 350 deep","No.",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"$f":"IF(E154 = CHAR(37), F154*G154/100,F154*G154)","v":{"v":0,"d":"0.00"}}]
[]
[25177,"4.1.9.18","8.2.6 (d)","Other than circular, up to and including 0.5m² up to 350 deep","No.",{"v":8,"d":"8.00"},{"v":0,"d":"0.00"},{"$f":"IF(E156 = CHAR(37), F156*G156/100,F156*G156)","v":{"v":0,"d":"0.00"}}]
[]
[25178,"4.1.9.19","8.2.6 (d)","Square up to and including 0,5m² up to 350 deep","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E158 = CHAR(37), F158*G158/100,F158*G158)","v":{"v":0,"d":"0.00"}}]
[]
[25179,"4.1.9.20",null,"Box-out special for temporary interconnecting of the outlet channel during operation of temporary bypass line, including coating of reinforcing as shown on the drawings.(60398/36)","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E160 = CHAR(37), F160*G160/100,F160*G160)","v":{"v":0,"d":"0.00"}}]
[]
[25180,"4.1.9.21",null,"Box-out special circular for temporary connection to the bypass line, including coating of reinforcing as shown on the drawings. (60398/36)","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E162 = CHAR(37), F162*G162/100,F162*G162)","v":{"v":0,"d":"0.00"}}]
[]
[25181,"4.1.10","8.1.2\r\nPSG 8.1.2","REINFORCING"]
[]
[25182,"4.1.10.1","8.3.1","High tensile Reinforcing bars up to 32mm dia.","t",{"v":23,"d":"23.00"},{"v":0,"d":"0.00"},{"$f":"IF(E166 = CHAR(37), F166*G166/100,F166*G166)","v":{"v":0,"d":"0.00"}}]
[]
[25183,"4.1.10.2","8.3.2","Mesh ref 888","m²",{"v":45,"d":"45.00"},{"v":0,"d":"0.00"},{"$f":"IF(E168 = CHAR(37), F168*G168/100,F168*G168)","v":{"v":0,"d":"0.00"}}]
[]
[25184,"4.1.11","8.1.3","CONCRETE"]
[]
[25266,"4.1.11.1","PSG 5.5.3.2","Concrete mix designs","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E172 = CHAR(37), F172*G172/100,F172*G172)","v":{"v":0,"d":"0.00"}}]
[]
[25185,null,null,"Blinding in 15MPa/19mm"]
[]
[25186,"4.1.11.2","8.4.2","50mm blinding below pile caps","m²",{"v":13,"d":"13.00"},{"v":0,"d":"0.00"},{"$f":"IF(E176 = CHAR(37), F176*G176/100,F176*G176)","v":{"v":0,"d":"0.00"}}]
[]
[25187,"4.1.11.3","8.4.2","50mm blinding under structure","m²",{"v":110,"d":"110.00"},{"v":0,"d":"0.00"},{"$f":"IF(E178 = CHAR(37), F178*G178/100,F178*G178)","v":{"v":0,"d":"0.00"}}]
[]
[25188,"4.1.11.4","8.4.2","50mm blinding under inlet/outlet channels/chambers","m²",{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"$f":"IF(E180 = CHAR(37), F180*G180/100,F180*G180)","v":{"v":0,"d":"0.00"}}]
[]
[25189,"4.1.11.5","8.4.2","50mm blinding under connecting channel","m²",{"v":17,"d":"17.00"},{"v":0,"d":"0.00"},{"$f":"IF(E182 = CHAR(37), F182*G182/100,F182*G182)","v":{"v":0,"d":"0.00"}}]
[]
[25190,null,"8.4.3","35MPa/19mm watertight concrete to:"]
[]
[25191,"4.1.11.6","8.4.3","Pile Caps","m³",{"v":7,"d":"7.00"},{"v":0,"d":"0.00"},{"$f":"IF(E186 = CHAR(37), F186*G186/100,F186*G186)","v":{"v":0,"d":"0.00"}}]
[]
[25192,"4.1.11.7","8.4.3","350mm floor slab to pile caps","m³",{"v":40,"d":"40.00"},{"v":0,"d":"0.00"},{"$f":"IF(E188 = CHAR(37), F188*G188/100,F188*G188)","v":{"v":0,"d":"0.00"}}]
[]
[25193,"4.1.11.8","8.4.3","Flocculation tank walls","m³",{"v":40,"d":"40.00"},{"v":0,"d":"0.00"},{"$f":"IF(E190 = CHAR(37), F190*G190/100,F190*G190)","v":{"v":0,"d":"0.00"}}]
[]
[25194,"4.1.11.9","8.4.3","Walkway slabs","m³",{"v":9,"d":"9.00"},{"v":0,"d":"0.00"},{"$f":"IF(E192 = CHAR(37), F192*G192/100,F192*G192)","v":{"v":0,"d":"0.00"}}]
[]
[25195,"4.1.11.10","8.4.3","Inlet chamber and channel","m³",{"v":23,"d":"23.00"},{"v":0,"d":"0.00"},{"$f":"IF(E194 = CHAR(37), F194*G194/100,F194*G194)","v":{"v":0,"d":"0.00"}}]
[]
[25196,"4.1.11.11","8.4.3","Outlet channel","m³",{"v":7,"d":"7.00"},{"v":0,"d":"0.00"},{"$f":"IF(E196 = CHAR(37), F196*G196/100,F196*G196)","v":{"v":0,"d":"0.00"}}]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H153:H197)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 4 - FLOCCULATION TANKS"]
[{"$nulls":7},"SECTION 4: FLOCCULATION TANKS"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H198","v":{"v":0,"d":"0.00"}}]
[25197,"4.1.11.12","8.4.3","Connecting channel","m³",{"v":9.5,"d":"9.50"},{"v":0,"d":"0.00"},{"$f":"IF(E203 = CHAR(37), F203*G203/100,F203*G203)","v":{"v":0,"d":"0.00"}}]
[]
[25198,null,null,"25MPa/19mm concrete to:"]
[]
[25199,"4.1.11.13","8.4.3","Stairs","m³",{"v":1.5,"d":"1.50"},{"v":0,"d":"0.00"},{"$f":"IF(E207 = CHAR(37), F207*G207/100,F207*G207)","v":{"v":0,"d":"0.00"}}]
[]
[25200,null,null,"15MPa/19mm concrete to:"]
[]
[25201,"4.1.11.14","8.4.3","Thickenings to temporary bypass line pipe","m³",0.75,{"v":0,"d":"0.00"},{"$f":"IF(E211 = CHAR(37), F211*G211/100,F211*G211)","v":{"v":0,"d":"0.00"}}]
[]
[25202,null,null,"No-fines concrete:"]
[]
[25203,"4.1.11.15","PSG 5.5.b11","No-fines concrete to toe of base slab as shown.","m³",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E215 = CHAR(37), F215*G215/100,F215*G215)","v":{"v":0,"d":"0.00"}}]
[]
[25204,null,null,"Special concrete:"]
[]
[25205,null,null,"45MPa no/low shrink quick set repair concrete to fill in temporary bypass box-outs (placed and cured under shut-down conditions). Side walls to be primed with dry to wet concrete primer, and a central bead of sikaswell (or similar approved). (Ref drawing 60398/36)"]
[]
[25206,"4.1.11.16",null,"Outlet channel interconnection box-out. ","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E221 = CHAR(37), F221*G221/100,F221*G221)","v":{"v":0,"d":"0.00"}}]
[]
[25207,"4.1.11.17",null,"Circular box out for temporary connection to the bypass line","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E223 = CHAR(37), F223*G223/100,F223*G223)","v":{"v":0,"d":"0.00"}}]
[]
[25208,"4.1.11.18",null,"Circular break-out in existing inlet channel for temporary connection to bypass line.","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E225 = CHAR(37), F225*G225/100,F225*G225)","v":{"v":0,"d":"0.00"}}]
[]
[25209,null,"8.4.4\r\nPSG 5.2.1","Unformed Surface Finish"]
[]
[25210,"4.1.11.19","8.4.4 (a)","Wood floated finish to base toe","m²",{"v":22,"d":"22.00"},{"v":0,"d":"0.00"},{"$f":"IF(E229 = CHAR(37), F229*G229/100,F229*G229)","v":{"v":0,"d":"0.00"}}]
[]
[25211,"4.1.11.20","8.4.4 (b)","Steel-floated finish to flocculation tank floor","m²",{"v":80,"d":"80.00"},{"v":0,"d":"0.00"},{"$f":"IF(E231 = CHAR(37), F231*G231/100,F231*G231)","v":{"v":0,"d":"0.00"}}]
[]
[25212,"4.1.11.21","8.4.4 (b)","Steel-floated finish to walkway slab","m²",{"v":55,"d":"55.00"},{"v":0,"d":"0.00"},{"$f":"IF(E233 = CHAR(37), F233*G233/100,F233*G233)","v":{"v":0,"d":"0.00"}}]
[]
[25213,"4.1.11.22","8.4.4 (b)","Steel-floated finish to top of walls (excluding sloped)","m²",{"v":17,"d":"17.00"},{"v":0,"d":"0.00"},{"$f":"IF(E235 = CHAR(37), F235*G235/100,F235*G235)","v":{"v":0,"d":"0.00"}}]
[]
[25214,"4.1.11.23","8.4.4 (b)","Steel-floated finish to inlet channel and chamber slab (excluding sloped)","m²",{"v":17,"d":"17.00"},{"v":0,"d":"0.00"},{"$f":"IF(E237 = CHAR(37), F237*G237/100,F237*G237)","v":{"v":0,"d":"0.00"}}]
[]
[25215,"4.1.11.24","8.4.4 (b)","Steel-floated finish to outlet channel slab","m²",{"v":12,"d":"12.00"},{"v":0,"d":"0.00"},{"$f":"IF(E239 = CHAR(37), F239*G239/100,F239*G239)","v":{"v":0,"d":"0.00"}}]
[]
[25216,"4.1.11.25","8.4.4 (b)","Steel-floated finish, sloped, to rapid mixing channel floor","m²",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E241 = CHAR(37), F241*G241/100,F241*G241)","v":{"v":0,"d":"0.00"}}]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H202:H241)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 4 - FLOCCULATION TANKS"]
[{"$nulls":7},"SECTION 4: FLOCCULATION TANKS"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H242","v":{"v":0,"d":"0.00"}}]
[25217,"4.1.11.26","8.4.4 (b)","Steel-floated finish, sloped, to rapid mixing channel walls","m²",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"$f":"IF(E247 = CHAR(37), F247*G247/100,F247*G247)","v":{"v":0,"d":"0.00"}}]
[]
[25218,"4.1.11.27","8.4.4 (b)","Steel-floated finish to connecting channel floor","m²",{"v":13,"d":"13.00"},{"v":0,"d":"0.00"},{"$f":"IF(E249 = CHAR(37), F249*G249/100,F249*G249)","v":{"v":0,"d":"0.00"}}]
[]
[25219,"4.1.11.28","8.4.4 (b)","Steel-floated finish to top of connecting channel walls","m²",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E251 = CHAR(37), F251*G251/100,F251*G251)","v":{"v":0,"d":"0.00"}}]
[]
[25267,"4.1.12","PSG 5.5.8\r\nPSG 8.4.7","CURING AND PROTECTION"]
[]
[25268,"4.1.12.1",null,"Flocculation Tank base","m²",{"v":16,"d":"16.00"},{"v":0,"d":"0.00"},{"$f":"IF(E255 = CHAR(37), F255*G255/100,F255*G255)","v":{"v":0,"d":"0.00"}}]
[]
[25269,"4.1.12.2",null,"Flocculation Tank walls","m²",{"v":280,"d":"280.00"},{"v":0,"d":"0.00"},{"$f":"IF(E257 = CHAR(37), F257*G257/100,F257*G257)","v":{"v":0,"d":"0.00"}}]
[]
[25270,"4.1.12.3",null,"Inlet channel and chamber walls","m²",{"v":120,"d":"120.00"},{"v":0,"d":"0.00"},{"$f":"IF(E259 = CHAR(37), F259*G259/100,F259*G259)","v":{"v":0,"d":"0.00"}}]
[]
[25271,"4.1.12.4",null,"Baffle walls","m²",{"v":12,"d":"12.00"},{"v":0,"d":"0.00"},{"$f":"IF(E261 = CHAR(37), F261*G261/100,F261*G261)","v":{"v":0,"d":"0.00"}}]
[]
[25272,"4.1.12.5",null,"Outlet channel","m²",{"v":32,"d":"32.00"},{"v":0,"d":"0.00"},{"$f":"IF(E263 = CHAR(37), F263*G263/100,F263*G263)","v":{"v":0,"d":"0.00"}}]
[]
[25273,"4.1.12.6",null,"Connecting channel","m²",{"v":43,"d":"43.00"},{"v":0,"d":"0.00"},{"$f":"IF(E265 = CHAR(37), F265*G265/100,F265*G265)","v":{"v":0,"d":"0.00"}}]
[]
[25274,"4.1.12.7",null,"Stairs","m²",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E267 = CHAR(37), F267*G267/100,F267*G267)","v":{"v":0,"d":"0.00"}}]
[]
[25275,"4.1.12.8",null,"Walkway edges","m²",{"v":9,"d":"9.00"},{"v":0,"d":"0.00"},{"$f":"IF(E269 = CHAR(37), F269*G269/100,F269*G269)","v":{"v":0,"d":"0.00"}}]
[]
[25276,"4.1.12.9",null,"Flocculation Tank base toe top","m²",{"v":22,"d":"22.00"},{"v":0,"d":"0.00"},{"$f":"IF(E271 = CHAR(37), F271*G271/100,F271*G271)","v":{"v":0,"d":"0.00"}}]
[]
[25277,"4.1.12.10",null,"Flocculation tank floor top","m²",{"v":80,"d":"80.00"},{"v":0,"d":"0.00"},{"$f":"IF(E273 = CHAR(37), F273*G273/100,F273*G273)","v":{"v":0,"d":"0.00"}}]
[]
[25278,"4.1.12.11",null,"Walkway slab top","m²",{"v":55,"d":"55.00"},{"v":0,"d":"0.00"},{"$f":"IF(E275 = CHAR(37), F275*G275/100,F275*G275)","v":{"v":0,"d":"0.00"}}]
[]
[25279,"4.1.12.12",null,"Top of walls","m²",{"v":30,"d":"30.00"},{"v":0,"d":"0.00"},{"$f":"IF(E277 = CHAR(37), F277*G277/100,F277*G277)","v":{"v":0,"d":"0.00"}}]
[]
[25280,"4.1.12.13",null,"Chamber slab","m²",{"v":12,"d":"12.00"},{"v":0,"d":"0.00"},{"$f":"IF(E279 = CHAR(37), F279*G279/100,F279*G279)","v":{"v":0,"d":"0.00"}}]
[]
[25281,"4.1.12.14",null,"Mixing channel floor","m²",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E281 = CHAR(37), F281*G281/100,F281*G281)","v":{"v":0,"d":"0.00"}}]
[]
[25282,"4.1.12.15",null,"Connecting channel floor","m²",{"v":13,"d":"13.00"},{"v":0,"d":"0.00"},{"$f":"IF(E283 = CHAR(37), F283*G283/100,F283*G283)","v":{"v":0,"d":"0.00"}}]
[]
[25220,"4.1.13",null,"JOINTS"]
[]
[25221,"4.1.13.1","8.5","200 x 2mm thick sikadur combiflex system or similar approved ","m",{"v":350,"d":"350.00"},{"v":0,"d":"0.00"},{"$f":"IF(E287 = CHAR(37), F287*G287/100,F287*G287)","v":{"v":0,"d":"0.00"}}]
[]
[25222,"4.1.13.2","8.5","250 x 3mm thick plasticized PVC type control waterbar with clips to reinforcing ","m",{"v":260,"d":"260.00"},{"v":0,"d":"0.00"},{"$f":"IF(E289 = CHAR(37), F289*G289/100,F289*G289)","v":{"v":0,"d":"0.00"}}]
[]
[25223,"4.1.13.3","8.5","\"Sikaswell P\" Extrudable Water swelling Profile joint sealing waterstop (Provisional)","m",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E291 = CHAR(37), F291*G291/100,F291*G291)","v":{"v":0,"d":"0.00"}}]
[]
[25224,"4.1.14","SANS 1200HA\r\nPSHA","STRUCTURAL STEELWORK"]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H246:H294)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 4 - FLOCCULATION TANKS"]
[{"$nulls":7},"SECTION 4: FLOCCULATION TANKS"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H295","v":{"v":0,"d":"0.00"}}]
[25225,"4.1.14.1","8.3.2","Supply, fabricate, deliver and install coated GMS ball type handrailing, Height & style to match existing. (including sloped as shown), complete.","m",{"v":160,"d":"160.00"},{"v":0,"d":"0.00"},{"$f":"IF(E300 = CHAR(37), F300*G300/100,F300*G300)","v":{"v":0,"d":"0.00"}}]
[]
[25226,"4.1.14.2","8.3.2","Supply, fabricate, deliver and install coated GMS ball type handrailing to existing clarifier wall. Height & style to match existing.","m",{"v":20,"d":"20.00"},{"v":0,"d":"0.00"},{"$f":"IF(E302 = CHAR(37), F302*G302/100,F302*G302)","v":{"v":0,"d":"0.00"}}]
[]
[25227,"4.1.14.3",null,"Swing gate to ball type handrailing as detailed ","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E304 = CHAR(37), F304*G304/100,F304*G304)","v":{"v":0,"d":"0.00"}}]
[]
[25228,"4.1.14.4",null,"Stainless steel ladder to flocculation tank walls to 2,5m high with extended lugs for handgrip","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E306 = CHAR(37), F306*G306/100,F306*G306)","v":{"v":0,"d":"0.00"}}]
[]
[25229,"4.1.14.5",null,"Supply, fabricate, deliver and install 40x40 GMS grating (40x3 bearer bar). Grating segments to be banded. Holes to manufactured for items such as hand railing stanchions, hand stop slits, and jib crane support.","m²",{"v":28,"d":"28.00"},{"v":0,"d":"0.00"},{"$f":"IF(E308 = CHAR(37), F308*G308/100,F308*G308)","v":{"v":0,"d":"0.00"}}]
[]
[25230,"4.1.14.6",null,"Supply, fabricate, deliver and install 50x50(x5mm) GMS support beam for grating, fixed to wall with galv. M12 chemical anchors at 300mm spacing","m",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E310 = CHAR(37), F310*G310/100,F310*G310)","v":{"v":0,"d":"0.00"}}]
[]
[25231,"4.1.14.7",null,"Supply, fabricate, deliver and cast in 40x40(x3mm) GMS support bracket for grating, cast in with fishtails at 300mm centres.","m",{"v":45,"d":"45.00"},{"v":0,"d":"0.00"},{"$f":"IF(E312 = CHAR(37), F312*G312/100,F312*G312)","v":{"v":0,"d":"0.00"}}]
[]
[25232,"4.1.15",null,"MISCELLANEOUS WORK"]
[]
[25233,null,null,"DRAINAGE"]
[]
[25234,"4.1.15.1",null,"110mm PVC Drain pipe under gully drain, laid to minimum 2% fall to daylight.","m",{"v":40,"d":"40.00"},{"v":0,"d":"0.00"},{"$f":"IF(E318 = CHAR(37), F318*G318/100,F318*G318)","v":{"v":0,"d":"0.00"}}]
[]
[25235,null,null,"DUCTS"]
[]
[25236,"4.1.15.2",null,"DN50 PN12 HDPE sleeves with SS draw wire","m",{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"$f":"IF(E322 = CHAR(37), F322*G322/100,F322*G322)","v":{"v":0,"d":"0.00"}}]
[]
[25237,null,null,"FIRE SAFETY"]
[]
[25238,"4.1.15.3",null,"Supply and install 9kg DCP fire extinguisher to wall, complete with weather cabinet and signage.","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E326 = CHAR(37), F326*G326/100,F326*G326)","v":{"v":0,"d":"0.00"}}]
[]
[25239,"4.1.15.4",null,"Supply and install 5kg CO2 fire extinguisher to wall, complete with weather cabinet and signage.","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E328 = CHAR(37), F328*G328/100,F328*G328)","v":{"v":0,"d":"0.00"}}]
[]
[25240,"4.1.16","PSG 7.3.9","TESTING AND COMMISSIONING "]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H299:H330)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 4 - FLOCCULATION TANKS"]
[{"$nulls":7},"SECTION 4: FLOCCULATION TANKS"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H331","v":{"v":0,"d":"0.00"}}]
[25241,"4.1.16.1",null,"Testing of flocculation tank for water tightness in accordance with the specifications.","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E336 = CHAR(37), F336*G336/100,F336*G336)","v":{"v":0,"d":"0.00"}}]
[]
[25242,"4.1.16.2",null,"Temporary blocking off the inlet chamber and testing for water tightness in accordance with the specifications ","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E338 = CHAR(37), F338*G338/100,F338*G338)","v":{"v":0,"d":"0.00"}}]
[]
[25243,"4.1.17","SANS 1200ME, MJ, MK, MF","SEGMENTED PAVED WALKWAY"]
[]
[25244,"4.1.17.1",null,"Compaction to 95% Mod AASHTO of 150mm thick insitu layer under C4 (priced below)","m²",{"v":45,"d":"45.00"},{"v":0,"d":"0.00"},{"$f":"IF(E342 = CHAR(37), F342*G342/100,F342*G342)","v":{"v":0,"d":"0.00"}}]
[]
[25245,"4.1.17.2","MF8.3.3-8","Supply from commercial sources, construct, stabilise with 4% cement 125mm thick gravel sub-base C4 layer compacted to 97% mod AASHTO","m²",{"v":45,"d":"45.00"},{"v":0,"d":"0.00"},{"$f":"IF(E344 = CHAR(37), F344*G344/100,F344*G344)","v":{"v":0,"d":"0.00"}}]
[]
[25246,"4.1.17.3","MK8.2.2","Supply, lay to levels and bed precast  concrete half-round drain 330mm wide","m",{"v":15,"d":"15.00"},{"v":0,"d":"0.00"},{"$f":"IF(E346 = CHAR(37), F346*G346/100,F346*G346)","v":{"v":0,"d":"0.00"}}]
[]
[25247,"4.1.17.4","MK8.2.2","Cast in situ segments with gully grid, complete with SS gully grid and sweep tee connection to drain pipe, in 20MPa/19mm concrete.","No.",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"$f":"IF(E348 = CHAR(37), F348*G348/100,F348*G348)","v":{"v":0,"d":"0.00"}}]
[]
[25248,"4.1.17.5","MK8.2.2","Cast in situ 200x200 concrete edge beam in 20MPa/19mm concrete","m",{"v":20,"d":"20.00"},{"v":0,"d":"0.00"},{"$f":"IF(E350 = CHAR(37), F350*G350/100,F350*G350)","v":{"v":0,"d":"0.00"}}]
[]
[25249,"4.1.17.6","MK8.2.2","Supply, lay and bed including 20mm sand bedding, jointing sand, and edge trimming as required, 60mm type S-A paving in herringbone.","m²",{"v":65,"d":"65.00"},{"v":0,"d":"0.00"},{"$f":"IF(E352 = CHAR(37), F352*G352/100,F352*G352)","v":{"v":0,"d":"0.00"}}]
[]
[25250,"4.1.18","SANS 1200L\r\nPSL","PIPEWORK"]
[]
[25251,null,null,"Rates to include necessary couplings, sockets, flange jointing material, cutting, welding, joining, lining, coating, and coating repair on site as necessary."]
[]
[25252,"4.1.18.1",null,"DN500 PN10 epoxy coated and lined flanged / bell ended (DN700) bend special to bypass line, with puddle.","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E358 = CHAR(37), F358*G358/100,F358*G358)","v":{"v":0,"d":"0.00"}}]
[]
[25253,"4.1.18.2",null,"DN500 PN10 epoxy coated and lined flanged / bell ended (DN700) pipe 3400 long to bypass line, with puddle.","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E360 = CHAR(37), F360*G360/100,F360*G360)","v":{"v":0,"d":"0.00"}}]
[]
[25254,"4.1.19","SANS 1200A","PROVISIONAL SUMS"]
[]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H335:H364)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 4 - FLOCCULATION TANKS"]
[{"$nulls":7},"SECTION 4: FLOCCULATION TANKS"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H365","v":{"v":0,"d":"0.00"}}]
[25255,"4.1.19.1","8.5 (a)","Provide the Provisional Sum of R25000 for signage and painting as instructed by the Engineer","Prov Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E370 = CHAR(37), F370*G370/100,F370*G370)","v":{"v":0,"d":"0.00"}}]
[]
[25256,"4.1.19.2",null,"Contractors markup on above","%",{"$f":"H370","v":{"v":0,"d":"0.00"}},{"v":0,"d":"0.00"},{"$f":"IF(E372 = CHAR(37), F372*G372/100,F372*G372)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":53}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H369:H425)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 4 - FLOCCULATION TANKS"]
[{"$nulls":3},"SUMMARY OF SECTIONS"]
[null," ","SECTION","DESCRIPTION",{"$nulls":3},"AMOUNT\n(RAND)"]
[null,null,"4.1","SECTION 4: FLOCCULATION TANKS",{"$nulls":3},{"$f":"H426","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":57}
[null,null," Total Carried Forward To Summary Of Schedules"," Total Carried Forward To Summary Of Schedules",{"$nulls":3},{"$f":"SUM(H430:H487)","v":{"v":0,"d":"0.00"}}]

{"sheet":"Schedule 5","index":4,"n_rows":299,"n_cols":8,"rows_kept":299}
["Rate=G","SCHEDULE 5 - WATERWORKS EQUIPMENT"]
[{"$nulls":7},"SECTION 5: WATERWORKS EQUIPMENT"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[25283,"5.1",null,"SECTION 5: WATERWORKS EQUIPMENT"]
[]
[25284,"5.1.1","PWW","WATERWORKS EQUIPMENT: PWW"]
[]
[25285,null,null,"HEAD OF WORKS EQUIPMENT (Ref Drawing 60398/35-60398/39)"]
[]
[25286,"5.1.1.1","PWW 8.1","Supply and install DN500 PN10 clockwise closing wedge gate valve with rising spindle (AIWC)","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E10 = CHAR(37), F10*G10/100,F10*G10)","v":{"v":0,"d":"0.00"}}]
[]
[25287,"5.1.1.2","PWW 8.2","Supply and install DN400 PN10 electromagnetic flowmeter (AIWC)","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E12 = CHAR(37), F12*G12/100,F12*G12)","v":{"v":0,"d":"0.00"}}]
[]
[25288,"5.1.1.3","PWW8.3,8.4","Supply and install DN500 PN10 knife gate valve complete with electric actuator suitable for flow modulation ","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E14 = CHAR(37), F14*G14/100,F14*G14)","v":{"v":0,"d":"0.00"}}]
[]
[25289,"5.1.1.4","PWW 9.1","Supply and install automated inclined stainless steel racked screen with bottom turnabout (Huber RakeMax or similar approved) complete with shaftless screw conveyor","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E16 = CHAR(37), F16*G16/100,F16*G16)","v":{"v":0,"d":"0.00"}}]
[]
[25290,"5.1.1.5","PWW 9.2","Supply and Install manually racked standby stainless steel screen","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E18 = CHAR(37), F18*G18/100,F18*G18)","v":{"v":0,"d":"0.00"}}]
[]
[25291,"5.1.1.6","PWW 9.3","Supply and install 500X500mm stainless steel penstock and frame (Penstock to be lockable in position)","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E20 = CHAR(37), F20*G20/100,F20*G20)","v":{"v":0,"d":"0.00"}}]
[]
[25292,"5.1.1.7","PWW 9.3","Supply and install 1.32x1.2m stainless steel penstock and frame","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E22 = CHAR(37), F22*G22/100,F22*G22)","v":{"v":0,"d":"0.00"}}]
[]
[25293,"5.1.1.8","PWW 9.3","Supply and install 1.12x0.7m stainless steel penstock and frame","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E24 = CHAR(37), F24*G24/100,F24*G24)","v":{"v":0,"d":"0.00"}}]
[]
[25294,"5.1.1.9","PWW 9.3","Supply and install 1.12x0.97m stainless steel penstock and frame","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E26 = CHAR(37), F26*G26/100,F26*G26)","v":{"v":0,"d":"0.00"}}]
[]
[25295,"5.1.1.10","PWW9.5","Supply and install ultrasonic depth indicator complete with DN300 PVC stilling well","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E28 = CHAR(37), F28*G28/100,F28*G28)","v":{"v":0,"d":"0.00"}}]
[]
[25296,"5.1.1.11","PWW 9.6","Supply, deliver and install inlet chamber weir plate (SS304L) for inlet level control and flow measurement, as detailed on the drawings.","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E30 = CHAR(37), F30*G30/100,F30*G30)","v":{"v":0,"d":"0.00"}}]
[]
[25297,"5.1.1.12","PWW 9.6","Supply, deliver and install 1200x200x2mm thick (SS304L) inlet weir plates to +/- 2mm level accuracy.","No.",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"$f":"IF(E32 = CHAR(37), F32*G32/100,F32*G32)","v":{"v":0,"d":"0.00"}}]
[]
[25298,"5.1.1.13","PWW13.2","Supply and install streaming current detector in IP67 wall mounted enclosure complete with sample pump and pipework","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E34 = CHAR(37), F34*G34/100,F34*G34)","v":{"v":0,"d":"0.00"}}]
[]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H4:H36)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 5 - WATERWORKS EQUIPMENT"]
[{"$nulls":7},"SECTION 5: WATERWORKS EQUIPMENT"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H37","v":{"v":0,"d":"0.00"}}]
[25299,"5.1.1.14","PWW 9.4","1,04x0.26m aluminium hand stop complete with frame and lifting hook as detailed. ","No.",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"$f":"IF(E42 = CHAR(37), F42*G42/100,F42*G42)","v":{"v":0,"d":"0.00"}}]
[]
[25300,"5.1.1.15","PWW 9.6","Extra over item above for bracket(by contractor) for storage of handstops when not in use ","No.",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"$f":"IF(E44 = CHAR(37), F44*G44/100,F44*G44)","v":{"v":0,"d":"0.00"}}]
[]
[25301,"5.1.1.16","PWW 9.3","Supply and install 1.0x0.7m stainless steel penstock and frame","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E46 = CHAR(37), F46*G46/100,F46*G46)","v":{"v":0,"d":"0.00"}}]
[]
[25302,"5.1.1.17","PWW 10.1","Supply, deliver and install vertical mechanical mixers with VSDs in flocculation tank, in accordance with specification.","No.",{"v":8,"d":"8.00"},{"v":0,"d":"0.00"},{"$f":"IF(E48 = CHAR(37), F48*G48/100,F48*G48)","v":{"v":0,"d":"0.00"}}]
[]
[25303,"5.1.1.18","SANS 1200HA\r\nPSHA","Design, supply, and install complete (SS316) swing jib crane to 200kg rated load, maximum x/500 deflection, complete with load test and certificate. (See drawings 60398/35 and 60398/36 for concept). ","No.",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"$f":"IF(E50 = CHAR(37), F50*G50/100,F50*G50)","v":{"v":0,"d":"0.00"}}]
[]
[25304,"5.1.1.19",null,"Supply removable / easy assembly hoist chain trolley (stainless steel) to the above jib crane, min. 200kg rated capacity","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E52 = CHAR(37), F52*G52/100,F52*G52)","v":{"v":0,"d":"0.00"}}]
[]
[25305,"5.1.1.20",null,"Supply chain block to min. 5m lifting height, rated to min. 200kg capacity.","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E54 = CHAR(37), F54*G54/100,F54*G54)","v":{"v":0,"d":"0.00"}}]
[]
[25306,"5.1.1.21",null,"Provisional sum for the provision of additional safety equipment and signage as directed by the Engineer.","Prov Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E56 = CHAR(37), F56*G56/100,F56*G56)","v":{"v":0,"d":"0.00"}}]
[]
[25307,"5.1.1.22",null,"Contractor's mark-up for overheads and profit on item above","%",{"$f":"H56","v":{"v":0,"d":"0.00"}},{"v":0,"d":"0.00"},{"$f":"IF(E58 = CHAR(37), F58*G58/100,F58*G58)","v":{"v":0,"d":"0.00"}}]
[]
[25308,"5.1.1.23",null,"Supply heavy duty platform trolley to minimum 200kg load capacity with minimum 350mm dia. Wheels (Min. 1.0mx0.6m platform size)","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E60 = CHAR(37), F60*G60/100,F60*G60)","v":{"v":0,"d":"0.00"}}]
[]
[25309,"5.1.2",null,"TEMPORARY BYPASS WORKS"]
[]
[25367,null,null,"(Ref Drawing 60398/36)"]
[]
[25310,"5.1.2.1",null,"Design, supply, and install (under shutdown conditions) complete temporary channel isolation plug (epoxy coated MS) to block backflow into existing inlet channel during operation of temporary bypass line from new flocculation tanks, as shown in concept on the drawings,  complete with all materials as required (sealants, epoxy bolts assemblies, etc).","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E66 = CHAR(37), F66*G66/100,F66*G66)","v":{"v":0,"d":"0.00"}}]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H41:H66)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 5 - WATERWORKS EQUIPMENT"]
[{"$nulls":7},"SECTION 5: WATERWORKS EQUIPMENT"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H67","v":{"v":0,"d":"0.00"}}]
[25311,"5.1.2.2",null,"Design, supply, and install complete temporary flocculation tank outlet plates (primary leak protection) to prevent water passing through to final flow path during operation of temporary bypass line, as shown in concept on the drawings,  complete with all materials as required (sealants, epoxy bolts assemblies, etc).","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E72 = CHAR(37), F72*G72/100,F72*G72)","v":{"v":0,"d":"0.00"}}]
[]
[25312,"5.1.3",null,"CLARIFIER COMPLEX"]
[]
[25368,null,null,"(Ref Drawing 60398/40)"]
[]
[25313,"5.1.3.1","PWW 11.1","Drain and clean Dortmund clarifiers","No.",{"v":6,"d":"6.00"},{"v":0,"d":"0.00"},{"$f":"IF(E78 = CHAR(37), F78*G78/100,F78*G78)","v":{"v":0,"d":"0.00"}}]
[]
[25314,"5.1.3.2","PWW11.2","Removal of redundant clarifier equipment, including asbestos cement launder pipes, sludge  hoppers, steel support structures etc to EWS stores or Municipal waste site as instructed, in accordance with applicable Health and Safety and Environmental legislation","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E80 = CHAR(37), F80*G80/100,F80*G80)","v":{"v":0,"d":"0.00"}}]
[]
[25315,"5.1.3.3",null,"Manufacture, supply, and install new sludge hopper/concentrator cone and launder support structure (Epoxy coated heavy duty galvanised structural steel grade S355) as shown on the drawings.  The rate shall cover the cost of preparing shop drawings, supply of all materials, fabrication, loading, transporting to site, off loading, erection, anchoring (chemical anchors) and supports, all fasteners, washers, isolation/bearing strips and bolt assemblies, temporary bracing as necessary, etc. complete.   ","No.",{"v":6,"d":"6.00"},{"v":0,"d":"0.00"},{"$f":"IF(E82 = CHAR(37), F82*G82/100,F82*G82)","v":{"v":0,"d":"0.00"}}]
[]
[25316,"5.1.3.4",null,"Extra over above for additional on-site Epoxy coating complete launder support assembly once installed, including prepping and coating galv. Bolts, touch ups, etc. Measured per clarifier. To be levelled to +/-2mm across all launders and including across all clarifiers.","No.",{"v":6,"d":"6.00"},{"v":0,"d":"0.00"},{"$f":"IF(E84 = CHAR(37), F84*G84/100,F84*G84)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":9}
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H71:H93)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 5 - WATERWORKS EQUIPMENT"]
[{"$nulls":7},"SECTION 5: WATERWORKS EQUIPMENT"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H94","v":{"v":0,"d":"0.00"}}]
[25317,"5.1.3.5",null,"Prepare shop drawings for approval, manufacture, supply, deliver, and install new launders (SS316) as detailed (each launder length to be seamless), to support structure and to walls as shown. No Ferro-magnetic metal to non Ferro-magnetic metal contact shall rely on insulation through coating only, and shall instead have proper isolating bearing/pad/etc. ","m",{"v":440,"d":"440.00"},{"v":0,"d":"0.00"},{"$f":"IF(E99 = CHAR(37), F99*G99/100,F99*G99)","v":{"v":0,"d":"0.00"}}]
[]
[25318,"5.1.3.6",null,"Design, submit for approval, manufacture, and installation of Non-ferro-magnetic (300 range) Stainless Steel pulley system as detailed on the drawings, including ss wire-rope, ss pulley blocks, ss wire-rope winch, and winch support. No Ferro-magnetic metal to non-ferro-magnetic metal contact shall rely on insulation through coating only, and shall instead have proper isolating bearing/pad/etc. design. To suit up to 8m lifting range.","No.",{"v":6,"d":"6.00"},{"v":0,"d":"0.00"},{"$f":"IF(E101 = CHAR(37), F101*G101/100,F101*G101)","v":{"v":0,"d":"0.00"}}]
[]
[25319,"5.1.3.7","PWW11.4","Deliver, supply and install new 2.5m diameter sludge hopper/concentrator complete as per specification including flexible pipe with couplings etc. complete. ","No.",{"v":6,"d":"6.00"},{"v":0,"d":"0.00"},{"$f":"IF(E103 = CHAR(37), F103*G103/100,F103*G103)","v":{"v":0,"d":"0.00"}}]
[]
[25320,"5.1.3.8",null,"Squaring off of Launder outlet holes, including breaking back concrete and trowel applied repair grout to suit new launder profile.","No.",{"v":48,"d":"48.00"},{"v":0,"d":"0.00"},{"$f":"IF(E105 = CHAR(37), F105*G105/100,F105*G105)","v":{"v":0,"d":"0.00"}}]
[]
[25321,"5.1.4",null,"FILTER COMPLEX "]
[]
[25322,"5.1.4.1","PWW 12.1","Supply, deliver and install new removable clear FRP/Perspex covers to clearwells.","No",{"v":6,"d":"6.00"},{"v":0,"d":"0.00"},{"$f":"IF(E109 = CHAR(37), F109*G109/100,F109*G109)","v":{"v":0,"d":"0.00"}}]
[]
[25323,"5.1.4.2","PWW12.2","Supply and install filter media depth indicator plates ","No.",{"v":6,"d":"6.00"},{"v":0,"d":"0.00"},{"$f":"IF(E111 = CHAR(37), F111*G111/100,F111*G111)","v":{"v":0,"d":"0.00"}}]
[]
[25324,"5.1.4.3","PWW12.3","Provide the Provisional sum of R200 000 for top-up of filter media","Prov Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E113 = CHAR(37), F113*G113/100,F113*G113)","v":{"v":0,"d":"0.00"}}]
[]
[25325,"5.1.4.4",null,"Contractor's mark-up for overheads and profit on item above","%",{"$f":"H113","v":{"v":0,"d":"0.00"}},{"v":0,"d":"0.00"},{"$f":"IF(E115 = CHAR(37), F115*G115/100,F115*G115)","v":{"v":0,"d":"0.00"}}]
[]
[25326,"5.1.4.5","PWW","Provide the Provisional Sum of R120 000 for the rehabilitation of inlet clack valves","Prov Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E117 = CHAR(37), F117*G117/100,F117*G117)","v":{"v":0,"d":"0.00"}}]
[]
[25327,"5.1.4.6",null,"Contractors mark-up for overheads and profits on item above","%",{"$f":"H117","v":{"v":0,"d":"0.00"}},{"v":0,"d":"0.00"},{"$f":"IF(E119 = CHAR(37), F119*G119/100,F119*G119)","v":{"v":0,"d":"0.00"}}]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H98:H120)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 5 - WATERWORKS EQUIPMENT"]
[{"$nulls":7},"SECTION 5: WATERWORKS EQUIPMENT"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H121","v":{"v":0,"d":"0.00"}}]
[25328,"5.1.5",null,"POLYMER SYSTEM - FILLING, STORAGE, DOSING, MONITORING AND CONTROL"]
[]
[25369,null,null,"(Ref Drawing 60398/41)"]
[]
[25329,"5.1.5.1","PWW13.1","Design, supply and install polymer storage and dosing facility complete as specified. The rate to also include for coring of concrete walls to accommodate pipework as per the Contractor's design and excavation and bedding for buried pipe between the dosing pumps and sparge pipe at the new inlet. ","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E130 = CHAR(37), F130*G130/100,F130*G130)","v":{"v":0,"d":"0.00"}}]
[]
[25330,"5.1.5.2",null,"Provide the Provisional sum of R35 000 for an allowance for refurbishment and or replacement of existing polymer dosing equipment and pipework's.","Prov Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E132 = CHAR(37), F132*G132/100,F132*G132)","v":{"v":0,"d":"0.00"}}]
[]
[25331,"5.1.5.3",null,"Contractor's mark-up for overheads and profit on item above","%",{"$f":"H132","v":{"v":0,"d":"0.00"}},{"v":0,"d":"0.00"},{"$f":"IF(E134 = CHAR(37), F134*G134/100,F134*G134)","v":{"v":0,"d":"0.00"}}]
[]
[25332,"5.1.5.4","PWW 13.2","Refurbish and deliver to stores existing Streaming Current Detector (SCD) complete","No",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E136 = CHAR(37), F136*G136/100,F136*G136)","v":{"v":0,"d":"0.00"}}]
[]
[25333,"5.1.5.5","PWW13.2","Supply and deliver to EWS stores new SCD sample pump as per that specified in PWW 13.2.","No",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E138 = CHAR(37), F138*G138/100,F138*G138)","v":{"v":0,"d":"0.00"}}]
[]
[25334,"5.1.5.6",null,"Provide the Provisional sum of R15 000 for the supply and deliver safety signage","Prov Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E140 = CHAR(37), F140*G140/100,F140*G140)","v":{"v":0,"d":"0.00"}}]
[]
[25335,"5.1.5.7",null,"Contractor's mark-up for overheads and profit on item above","%",{"$f":"H140","v":{"v":0,"d":"0.00"}},{"v":0,"d":"0.00"},{"$f":"IF(E142 = CHAR(37), F142*G142/100,F142*G142)","v":{"v":0,"d":"0.00"}}]
[]
[25336,"5.1.5.8","PWW13.1","Testing and commissioning of the existing and new polymer dosing system.","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E144 = CHAR(37), F144*G144/100,F144*G144)","v":{"v":0,"d":"0.00"}}]
[]
[25370,"5.1.5.9",null,"Supply and install backflow prevention valve on the polymer dosing motive water supply line.","No",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E146 = CHAR(37), F146*G146/100,F146*G146)","v":{"v":0,"d":"0.00"}}]
[]
[25337,"5.1.6",null,"DISINFECTION - CHLORINE SYSTEM"]
[]
[25338,"5.1.6.1","PWW 13.3a","Supply, deliver and install new standby chlorinator and associated works complete as specified to the \"Vacuum Room\".","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E150 = CHAR(37), F150*G150/100,F150*G150)","v":{"v":0,"d":"0.00"}}]
[]
[]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H125:H153)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 5 - WATERWORKS EQUIPMENT"]
[{"$nulls":7},"SECTION 5: WATERWORKS EQUIPMENT"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H154","v":{"v":0,"d":"0.00"}}]
[25339,"5.1.6.2","PWW 13.3b","Supply, deliver and install new DN50 Class 12 chlorine dosing pipework from the existing chlorine room to the new head of works, including all excavation, bedding, backfill, pipework, bends, valves, couplings, connections, pipe supports and DN50 Class 12 PVC perforated sparge pipe and tie into motive water system complete as specified.","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E159 = CHAR(37), F159*G159/100,F159*G159)","v":{"v":0,"d":"0.00"}}]
[]
[25340,"5.1.6.3",null,"Provision sum for the provision of additional safety equipment and signage to improve the safety of the installation as directed by the Engineer.","Prov Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E161 = CHAR(37), F161*G161/100,F161*G161)","v":{"v":0,"d":"0.00"}}]
[]
[25341,"5.1.6.4",null,"Contractor's mark-up for overheads and profit on item above","%",{"$f":"H161","v":{"v":0,"d":"0.00"}},{"v":0,"d":"0.00"},{"$f":"IF(E163 = CHAR(37), F163*G163/100,F163*G163)","v":{"v":0,"d":"0.00"}}]
[]
[25342,"5.1.6.5","PWW 13.3","Allowance for the assessment, testing, report, recommendation, rehabilitation/servicing of the existing chlorine dosing system. Including for the testing, servicing, and calibration of the existing load cells for the 1t chlorine tanks. ","Prov Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E165 = CHAR(37), F165*G165/100,F165*G165)","v":{"v":0,"d":"0.00"}}]
[]
[25343,"5.1.6.6",null,"Contractor's mark-up for overheads and profit on item above","%",{"$f":"H165","v":{"v":0,"d":"0.00"}},{"v":0,"d":"0.00"},{"$f":"IF(E167 = CHAR(37), F167*G167/100,F167*G167)","v":{"v":0,"d":"0.00"}}]
[]
[25344,"5.1.6.7",null,"Facilitation of HAZOP study and preparation of report as specified.","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E169 = CHAR(37), F169*G169/100,F169*G169)","v":{"v":0,"d":"0.00"}}]
[]
[25345,"5.1.6.8",null,"Facilitation of MHI study and preparation of report as specified.","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E171 = CHAR(37), F171*G171/100,F171*G171)","v":{"v":0,"d":"0.00"}}]
[]
[25346,"5.1.6.9",null,"Civil works for bollard protection and chain at chlorine house to protect from skip loading/unloading etc.","Prov Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E173 = CHAR(37), F173*G173/100,F173*G173)","v":{"v":0,"d":"0.00"}}]
[]
[25371,"5.1.6.10",null,"Supply and install backflow prevention valve on the chlorine dosing motive water supply line.","No",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E175 = CHAR(37), F175*G175/100,F175*G175)","v":{"v":0,"d":"0.00"}}]
[]
[25347,"5.1.7",null,"MEASUREMENT OF KEY DETERMINANDS"]
[]
[25348,null,null,"Supply and install online analysers complete with sample pump, sample pipework, rotameter etc. complete as specified to:"]
[]
[25349,"5.1.7.1","PWW14.1","Turbidity: Raw Water","No",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E181 = CHAR(37), F181*G181/100,F181*G181)","v":{"v":0,"d":"0.00"}}]
[]
[25350,"5.1.7.2","PWW14.2","pH: Raw Water","No",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E183 = CHAR(37), F183*G183/100,F183*G183)","v":{"v":0,"d":"0.00"}}]
[]
[25351,"5.1.7.3","PWW14.3","Conductivity: Raw Water","No",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E185 = CHAR(37), F185*G185/100,F185*G185)","v":{"v":0,"d":"0.00"}}]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H158:H185)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 5 - WATERWORKS EQUIPMENT"]
[{"$nulls":7},"SECTION 5: WATERWORKS EQUIPMENT"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H186","v":{"v":0,"d":"0.00"}}]
[25352,"5.1.7.4","PWW14.4","Free Chlorine: Clarified Water","No",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E191 = CHAR(37), F191*G191/100,F191*G191)","v":{"v":0,"d":"0.00"}}]
[]
[25353,"5.1.7.5","PWW14.5","Turbidity: Clarified Water","No",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E193 = CHAR(37), F193*G193/100,F193*G193)","v":{"v":0,"d":"0.00"}}]
[]
[25354,"5.1.7.6","PWW14.6","Turbidity: Filtered Water","No",{"v":6,"d":"6.00"},{"v":0,"d":"0.00"},{"$f":"IF(E195 = CHAR(37), F195*G195/100,F195*G195)","v":{"v":0,"d":"0.00"}}]
[]
[25355,"5.1.7.7","PWW14.7","Turbidity: Potable Water","No",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E197 = CHAR(37), F197*G197/100,F197*G197)","v":{"v":0,"d":"0.00"}}]
[]
[25356,"5.1.7.8","PWW14.8","pH: Potable Water","No",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E199 = CHAR(37), F199*G199/100,F199*G199)","v":{"v":0,"d":"0.00"}}]
[]
[25357,"5.1.7.9","PWW14.10","Free Chlorine: Potable Water","No",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E201 = CHAR(37), F201*G201/100,F201*G201)","v":{"v":0,"d":"0.00"}}]
[]
[25358,"5.1.8",null,"REVIEW FOR COMPLIANCE"]
[]
[25359,"5.1.8.1",null,"Preparation of shop drawings and \"goodness of fit\" of mechanical pipework and fittings","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E205 = CHAR(37), F205*G205/100,F205*G205)","v":{"v":0,"d":"0.00"}}]
[]
[25360,"5.1.8.2",null,"Provision of laboratory equipment","Prov Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E207 = CHAR(37), F207*G207/100,F207*G207)","v":{"v":0,"d":"0.00"}}]
[]
[25361,"5.1.8.3",null,"Contractor's mark-up for overheads and profit on item above","%",{"$f":"H207","v":{"v":0,"d":"0.00"}},{"v":0,"d":"0.00"},{"$f":"IF(E209 = CHAR(37), F209*G209/100,F209*G209)","v":{"v":0,"d":"0.00"}}]
[]
[25362,"5.1.9",null,"ASSET MANAGEMENT AND PROVISION OF LIST OF SPARES"]
[]
[25363,"5.1.9.1",null,"Provision for critical spares","Prov Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E213 = CHAR(37), F213*G213/100,F213*G213)","v":{"v":0,"d":"0.00"}}]
[]
[25364,"5.1.9.2",null,"Contractor's mark-up for overheads and profit on item above","%",{"$f":"H213","v":{"v":0,"d":"0.00"}},{"v":0,"d":"0.00"},{"$f":"IF(E215 = CHAR(37), F215*G215/100,F215*G215)","v":{"v":0,"d":"0.00"}}]
[]
[25365,"5.1.9.3",null,"Provision for the supply and delivery of chemicals required for the dosing systems at the water treatment works for continuous operation over the 6 months trial period.","Prov Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E217 = CHAR(37), F217*G217/100,F217*G217)","v":{"v":0,"d":"0.00"}}]
[]
[25366,"5.1.9.4",null,"Contractor's mark-up for overheads and profit on item above","%",{"$f":"H217","v":{"v":0,"d":"0.00"}},{"v":0,"d":"0.00"},{"$f":"IF(E219 = CHAR(37), F219*G219/100,F219*G219)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":17}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H190:H236)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 5 - WATERWORKS EQUIPMENT"]
[{"$nulls":3},"SUMMARY OF SECTIONS"]
[null," ","SECTION","DESCRIPTION",{"$nulls":3},"AMOUNT\n(RAND)"]
[null,null,"5.1","SECTION 5: WATERWORKS EQUIPMENT",{"$nulls":3},{"$f":"H237","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":57}
[null,null," Total Carried Forward To Summary Of Schedules"," Total Carried Forward To Summary Of Schedules",{"$nulls":3},{"$f":"SUM(H241:H298)","v":{"v":0,"d":"0.00"}}]

{"sheet":"Schedule 6","index":5,"n_rows":1202,"n_cols":8,"rows_kept":1202}
["Rate=G","SCHEDULE 6 - ADMINISTRATION BUILDING EXTENSION"]
[{"$nulls":7},"SECTION 6.1: ALTERATIONS"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[20905,"6.1",null,"ALTERATIONS"]
[]
[20906,null,null,"NOTES:"]
[]
[20907,null,null,"Items described as to be re-used or to be handed over to the Client are to be carefully dismantled where necessary and stacked on site where directed, and the Contractor will be responsible for their removal and storage until required, and shall make good all items missing, damaged or broken at his own expense. All works references Dwgs 60398/11"]
[]
[21189,null,null,"Alterations to the fabric of existing structures will be executed in stages concurrently with the construction of the new work to ensure that the waterproofing integrity of the structures is maintained."]
[]
[20908,null,null,"Unless otherwise described, no materials from the alterations shall be re-used in any new work without the written approval of the client, with the exception of facing bricks required in filling to openings, etc., which may be re-used if free of cracks and chips and properly cleaned of all mortar"]
[]
[20909,null,null,"The Contractor is to take all dimensions affecting the existing buildings on the site as he will be solely responsible for all new work being to the correct sizes. The Engineer's Representative is to be notified immediately of any discrepancies between the drawings and the existing work and all work affected by these discrepancies is to be suspended until such time as the Engineer's Representative shall authorise its continuance"]
[]
[20913,null,null,"Prices are to include for carting away from site all materials not specifically mentioned as being stored on site for re-use or handed over to the client and all rubbish, debris, etc., arising from the alterations, etc., and for making good all work damaged or disturbed to the approval of the client"]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H4:H17)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 6 - ADMINISTRATION BUILDING EXTENSION"]
[{"$nulls":7},"SECTION 6.1: ALTERATIONS"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H18","v":{"v":0,"d":"0.00"}}]
[20914,null,null,"Tenderers are to include in pricing for the statutory requirements with regard to the demolition and disposal of asbestos cement material arising from the works"]
[]
[20915,"6.1.1",null,"GENERAL "]
[]
[20916,"6.1.1.1",null,"Allow for protecting all existing work liable to suffer damage (i.e. walls, finishes, floors, windows, etc.) from damage during the building operations, alterations, etc., and make good all work damaged with new material to match existing to the approval of the client","Sum",{"v":1,"d":"1.0"},{"v":0,"d":"0.00"},{"$f":"IF(E27 = CHAR(37), F27*G27/100,F27*G27)","v":{"v":0,"d":"0.00"}}]
[]
[20917,"6.1.1.2",null,"Dust screens of minimum height 3000mm (equal height throughout), between concrete floor and ceiling, roof slab, or floor slab above, of suitable timber framing with 375 micron polyethylene sheeting fixed on one side, including corners, ends, and any other intermediate posts and bracing as may be required for support, stability, etc","m",{"v":10,"d":"10.0"},{"v":0,"d":"0.00"},{"$f":"IF(E29 = CHAR(37), F29*G29/100,F29*G29)","v":{"v":0,"d":"0.00"}}]
[]
[20918,"6.1.2",null,"REMOVAL OF EXISTING WORK "]
[]
[20919,null,null,"Breaking down and removing brickwork etc"]
[]
[20920,"6.1.2.1",null,"Single skin wall","m²",{"v":15,"d":"15.0"},{"v":0,"d":"0.00"},{"$f":"IF(E35 = CHAR(37), F35*G35/100,F35*G35)","v":{"v":0,"d":"0.00"}}]
[]
[20921,null,null,"Taking out and removing doors, windows, etc., from brickwork to remain (building up or altering opening elsewhere measured)"]
[]
[21081,"6.1.2.2",null,"Hardwood single door and frame not exceeding 2,5m²\r\n","No.",{"v":6,"d":"6.0"},{"v":0,"d":"0.00"},{"$f":"IF(E39 = CHAR(37), F39*G39/100,F39*G39)","v":{"v":0,"d":"0.00"}}]
[]
[20922,"6.1.2.3",null,"Glazed steel window not exceeding 2,5m²","No.",{"v":6,"d":"6.0"},{"v":0,"d":"0.00"},{"$f":"IF(E41 = CHAR(37), F41*G41/100,F41*G41)","v":{"v":0,"d":"0.00"}}]
[]
[20923,null,null,"Taking out doors, windows, etc including thresholds, sills, etc from brickwork to be demolished and stored for reuse as directed by the Engineer."]
[]
[20924,"6.1.2.4",null,"Soap dispenser from brick walls","No.",{"v":2,"d":"2.0"},{"v":0,"d":"0.00"},{"$f":"IF(E45 = CHAR(37), F45*G45/100,F45*G45)","v":{"v":0,"d":"0.00"}}]
[]
[20925,"6.1.2.5",null,"Taking out and removing sundry joinery work, fittings, etc. ","No.",{"v":10,"d":"10.0"},{"v":0,"d":"0.00"},{"$f":"IF(E47 = CHAR(37), F47*G47/100,F47*G47)","v":{"v":0,"d":"0.00"}}]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H22:H48)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 6 - ADMINISTRATION BUILDING EXTENSION"]
[{"$nulls":7},"SECTION 6.1: ALTERATIONS"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H49","v":{"v":0,"d":"0.00"}}]
[21082,"6.1.2.6",null,"Change room bench from wall","No.",{"v":2,"d":"2.0"},{"v":0,"d":"0.00"},{"$f":"IF(E54 = CHAR(37), F54*G54/100,F54*G54)","v":{"v":0,"d":"0.00"}}]
[]
[20926,"6.1.2.7",null,"Existing lab chipboard cupboards and doors","m",{"v":6,"d":"6.0"},{"v":0,"d":"0.00"},{"$f":"IF(E56 = CHAR(37), F56*G56/100,F56*G56)","v":{"v":0,"d":"0.00"}}]
[]
[20927,null,null,"Hacking up/off and removing ceramic tile floor finishes including removing mortar bed or backing and preparing concrete or brick surfaces for new screed, plaster or tile finishes (elsewhere measured) "]
[]
[20928,"6.1.2.8",null,"Ceramic tiles on floors","m²",{"v":50,"d":"50.0"},{"v":0,"d":"0.00"},{"$f":"IF(E60 = CHAR(37), F60*G60/100,F60*G60)","v":{"v":0,"d":"0.00"}}]
[]
[20929,null,null,"Hacking up/off and removing white glazed tile wall finishes including removing mortar bed or backing and preparing concrete or brick surfaces for new screed, plaster or tile finishes (elsewhere measured) "]
[]
[20930,"6.1.2.9",null,"White glazed ceramic tiles to walls","m²",{"v":20,"d":"20.0"},{"v":0,"d":"0.00"},{"$f":"IF(E64 = CHAR(37), F64*G64/100,F64*G64)","v":{"v":0,"d":"0.00"}}]
[]
[20931,null,null,"Taking out and removing piping, sanitary fittings, etc. including disconnecting piping and stopping off fittings and making good floor and wall finishes (new tiling and paintwork elsewhere measured) "]
[]
[20932,"6.1.2.10",null,"Water supply pipework including fittings not exceeding 75mm diameter, inclusive of ancillary works","m",{"v":75,"d":"75.0"},{"v":0,"d":"0.00"},{"$f":"IF(E68 = CHAR(37), F68*G68/100,F68*G68)","v":{"v":0,"d":"0.00"}}]
[]
[20933,"6.1.2.11",null,"Stainless steel double bowl sink and drainer including fittings, etc, inclusive of ancillary works","No.",{"v":1,"d":"1.0"},{"v":0,"d":"0.00"},{"$f":"IF(E70 = CHAR(37), F70*G70/100,F70*G70)","v":{"v":0,"d":"0.00"}}]
[]
[20934,"6.1.2.12",null,"Ceramic wash hand basin, including short lengths of piping, fittings, etc, inclusive of ancillary works","No.",{"v":2,"d":"2.0"},{"v":0,"d":"0.00"},{"$f":"IF(E72 = CHAR(37), F72*G72/100,F72*G72)","v":{"v":0,"d":"0.00"}}]
[]
[21223,"6.1.2.13",null,"Urinal, inclusive of ancillary works","No.",{"v":2,"d":"2.0"},{"v":0,"d":"0.00"},{"$f":"IF(E74 = CHAR(37), F74*G74/100,F74*G74)","v":{"v":0,"d":"0.00"}}]
[]
[21224,"6.1.2.14",null,"Shower, inclusive of ancillary works","No.",{"v":1,"d":"1.0"},{"v":0,"d":"0.00"},{"$f":"IF(E76 = CHAR(37), F76*G76/100,F76*G76)","v":{"v":0,"d":"0.00"}}]
[]
[20935,null,null,"Taking out and removing glass and mirrors "]
[]
[20936,"6.1.2.15",null,"Mirror 1300 x 1500mm high from wall","No.",{"v":1,"d":"1.0"},{"v":0,"d":"0.00"},{"$f":"IF(E80 = CHAR(37), F80*G80/100,F80*G80)","v":{"v":0,"d":"0.00"}}]
[]
[23798,null,null,"Breaking down, cutting, and removal of brickwork "]
[]
[23799,"6.1.2.16",null,"Windows & Doors","m²",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E84 = CHAR(37), F84*G84/100,F84*G84)","v":{"v":0,"d":"0.00"}}]
[]
[20937,"6.1.3","PABR","BUILDING UP OPENINGS "]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H53:H87)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 6 - ADMINISTRATION BUILDING EXTENSION"]
[{"$nulls":7},"SECTION 6.1: ALTERATIONS"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H88","v":{"v":0,"d":"0.00"}}]
[20938,null,null,"External facebrick in Roan Satin FBX and internal common brick NFP for plaster and paint finish, brickwork in class II mortar in building up openings, including bonding new to existing and making good cement plaster (making good paintwork elsewhere)"]
[]
[20939,"6.1.3.1",null,"External facebrick","m²",{"v":20,"d":"20.0"},{"v":0,"d":"0.00"},{"$f":"IF(E95 = CHAR(37), F95*G95/100,F95*G95)","v":{"v":0,"d":"0.00"}}]
[]
[20940,"6.1.3.2",null,"Internal common brick","m²",{"v":20,"d":"20.0"},{"v":0,"d":"0.00"},{"$f":"IF(E97 = CHAR(37), F97*G97/100,F97*G97)","v":{"v":0,"d":"0.00"}}]
[]
[20941,null,null,"Internal common brick NFP in class II mortar in building up openings, including bonding new to existing and making good cement plaster on both sides (making good paintwork elsewhere)"]
[]
[20942,"6.1.3.3",null,"Single skin walls","m²",{"v":10,"d":"10.0"},{"v":0,"d":"0.00"},{"$f":"IF(E101 = CHAR(37), F101*G101/100,F101*G101)","v":{"v":0,"d":"0.00"}}]
[]
[20943,"6.1.3.4",null,"Double skin walls","m²",{"v":10,"d":"10.0"},{"v":0,"d":"0.00"},{"$f":"IF(E103 = CHAR(37), F103*G103/100,F103*G103)","v":{"v":0,"d":"0.00"}}]
[]
[20944,null,null,"Sundries "]
[]
[20945,"6.1.3.5",null,"Cutting, toothing and bonding new brick walls to existing brick walls","m²",{"v":40,"d":"40.0"},{"v":0,"d":"0.00"},{"$f":"IF(E107 = CHAR(37), F107*G107/100,F107*G107)","v":{"v":0,"d":"0.00"}}]
[]
[20946,"6.1.4","PABR","PREPARATORY WORK TO EXISTING SURFACES "]
[]
[20947,null,null,"Preparatory work to existing surfaces "]
[]
[20948,"6.1.4.1",null,"Making good to walls where white glazed tiles removed to receive new finish (Elsewhere measured)","m²",{"v":20,"d":"20.0"},{"v":0,"d":"0.00"},{"$f":"IF(E113 = CHAR(37), F113*G113/100,F113*G113)","v":{"v":0,"d":"0.00"}}]
[]
[20949,"6.1.4.2",null,"Making good to floors where ceramic tiles removed to receive new floor finish (Elsewhere measured)","m²",{"v":50,"d":"50.0"},{"v":0,"d":"0.00"},{"$f":"IF(E115 = CHAR(37), F115*G115/100,F115*G115)","v":{"v":0,"d":"0.00"}}]
[]
[20950,"6.1.4.3",null,"Remove paint and plaster surface from existing walls","m²",{"v":120,"d":"120.0"},{"v":0,"d":"0.00"},{"$f":"IF(E117 = CHAR(37), F117*G117/100,F117*G117)","v":{"v":0,"d":"0.00"}}]
[]
[20951,"6.1.5",null,"OPENINGS THROUGH EXISTING WALLS ETC "]
{"$rows_empty":10}
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H92:H129)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 6 - ADMINISTRATION BUILDING EXTENSION"]
[{"$nulls":7},"SECTION 6.1: ALTERATIONS"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H130","v":{"v":0,"d":"0.00"}}]
[20952,null,null,"Breaking out for and forming openings through brick walls for new doors and frames, including pre-stressed concrete lintels, making good cement plaster on both sides and into reveals and with 20 MPa concrete thresholds with steel trowelled finish (new doors and frames and making good paintwork elsewhere) "]
[]
[20953,"6.1.5.1",null,"Opening for door with timber frame 915 x 2134mm high overall through half brick wall","No.",{"v":1,"d":"1.0"},{"v":0,"d":"0.00"},{"$f":"IF(E137 = CHAR(37), F137*G137/100,F137*G137)","v":{"v":0,"d":"0.00"}}]
[]
[23793,"6.1.6","PABR","BRICKWORK SUNDRIES"]
[]
[23794,null,null,"Brick on edge lintels (into existing structure)"]
[]
[23795,"6.1.6.1",null,"110 x 150mm lintels in lengths not exceeding 3m","m",{"v":12,"d":"12.00"},{"v":0,"d":"0.00"},{"$f":"IF(E143 = CHAR(37), F143*G143/100,F143*G143)","v":{"v":0,"d":"0.00"}}]
[]
[23796,null,null,"Brick on edge sills (into existing structure)"]
[]
[23797,"6.1.6.2",null,"110 x 150mm sills in lengths not exceeding 3m","m",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E147 = CHAR(37), F147*G147/100,F147*G147)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":30}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H134:H177)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 6 - ADMINISTRATION BUILDING EXTENSION"]
[{"$nulls":7},"SECTION 6.2: CONCRETE, FORMWORK AND REINFORCING"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[20954,"6.2","SANS 1200 G, PSG","CONCRETE, FORMWORK, AND REINFORCING"]
[]
[21109,null,null,"SUPPLEMENTARY PREAMBLES:"]
[]
[20961,null,null,"Cost of tests"]
[]
[20962,null,null,"The costs of making, storing and testing of concrete test cubes as required under clause 7 \"Tests\" of SANS 1200 G shall include the cost of providing cube moulds necessary for the purpose, for testing costs and for submitting reports on the tests to the Engineer. The testing shall be undertaken by an independent firm or institution nominated by the contractor to the approval of the Engineer. (Test cubes are measured separately)"]
[]
[20963,null,null,"Formwork"]
[]
[20964,null,null,"Descriptions of formwork shall be deemed to include use and waste only (except where described as \"left in\" or \"permanent\"), for fitting together in the required forms, wedging, plumbing and fixing to true angles and surfaces as necessary to ensure easy release during stripping and for reconditioning as necessary before re-use"]
[]
[20965,null,null,"The vertical strutting shall be carried down to such construction as is sufficiently strong to afford the required support without damage and shall remain in position until the newly constructed work is able to support itself"]
[]
[20966,null,null,"Formwork to soffits of solid slabs etc shall be deemed to be to slabs not exceeding 250mm thick unless otherwise described"]
[]
[20967,null,null,"Formwork to soffits of slabs, beams, etc shall be deemed to be propped up exceeding 1,5m and not exceeding 3,5m high unless otherwise described"]
[]
[]
[]
[]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H182:H203)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 6 - ADMINISTRATION BUILDING EXTENSION"]
[{"$nulls":7},"SECTION 6.2: CONCRETE, FORMWORK AND REINFORCING"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H204","v":{"v":0,"d":"0.00"}}]
[20968,null,null,"Formwork to sides of bases, ground beams, etc will only be measured where it is prescribed by the engineer for design reasons. Formwork necessitated by irregularity or collapse of excavated faces will not be measured and the cost thereof shall be deemed to be included in the allowance for taking the risk of collapse of the sides of the excavations, provision for which is made in \"Earthworks\""]
[]
[20970,"6.2.1","8.4.3","REINFORCED CONCRETE"]
[]
[21155,"6.2.1.1","PSG 5.5.3.2","Concrete mix design","Sum",{"v":1,"d":"1.0"},{"v":0,"d":"0.00"},{"$f":"IF(E213 = CHAR(37), F213*G213/100,F213*G213)","v":{"v":0,"d":"0.00"}}]
[]
[20971,null,"8.4.3\r\nPSG5.5","Slabs in 25MPa/19mm stone"]
[]
[20972,"6.2.1.2",null,"200mm thick roof slab","m³",{"v":34,"d":"34.0"},{"v":0,"d":"0.00"},{"$f":"IF(E217 = CHAR(37), F217*G217/100,F217*G217)","v":{"v":0,"d":"0.00"}}]
[]
[20973,"6.2.1.3",null,"260mm thick floor slab","m³",{"v":29,"d":"29.0"},{"v":0,"d":"0.00"},{"$f":"IF(E219 = CHAR(37), F219*G219/100,F219*G219)","v":{"v":0,"d":"0.00"}}]
[]
[21083,"6.2.1.4",null,"200mm thick new walkway","m³",{"v":10,"d":"10.0"},{"v":0,"d":"0.00"},{"$f":"IF(E221 = CHAR(37), F221*G221/100,F221*G221)","v":{"v":0,"d":"0.00"}}]
[]
[21104,"6.2.1.5",null,"600mm thick wall beam","m³",{"v":4,"d":"4.0"},{"v":0,"d":"0.00"},{"$f":"IF(E223 = CHAR(37), F223*G223/100,F223*G223)","v":{"v":0,"d":"0.00"}}]
[]
[20910,"6.2.1.6",null,"400mm thick floor beam","m³",{"v":5,"d":"5.0"},{"v":0,"d":"0.00"},{"$f":"IF(E225 = CHAR(37), F225*G225/100,F225*G225)","v":{"v":0,"d":"0.00"}}]
[]
[22462,"6.2.1.7",null,"Columns","m³",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E227 = CHAR(37), F227*G227/100,F227*G227)","v":{"v":0,"d":"0.00"}}]
[]
[20975,"6.2.2","8.2, PSG 8.2.2","SMOOTH FORMWORK"]
[]
[20976,null,null,"Smooth finishes from formwork on:"]
[]
[21084,null,"8.2.2, PSG 8.2.2","Vertical plane to:"]
[]
[20977,"6.2.2.1",null,"Roof beam, external (long side)","m²",{"v":21,"d":"21.0"},{"v":0,"d":"0.00"},{"$f":"IF(E235 = CHAR(37), F235*G235/100,F235*G235)","v":{"v":0,"d":"0.00"}}]
[]
[20978,"6.2.2.2",null,"Roof beam, internal  (long side)","m²",{"v":21,"d":"21.0"},{"v":0,"d":"0.00"},{"$f":"IF(E237 = CHAR(37), F237*G237/100,F237*G237)","v":{"v":0,"d":"0.00"}}]
[]
[20979,"6.2.2.3",null,"Roof beam, external (short side)","m²",{"v":9,"d":"9.0"},{"v":0,"d":"0.00"},{"$f":"IF(E239 = CHAR(37), F239*G239/100,F239*G239)","v":{"v":0,"d":"0.00"}}]
[]
[20980,"6.2.2.4",null,"Roof beams, internal (short side)","m²",{"v":8,"d":"8.0"},{"v":0,"d":"0.00"},{"$f":"IF(E241 = CHAR(37), F241*G241/100,F241*G241)","v":{"v":0,"d":"0.00"}}]
[]
[20981,"6.2.2.5",null,"400mm, beam (external)","m²",{"v":17,"d":"17.0"},{"v":0,"d":"0.00"},{"$f":"IF(E243 = CHAR(37), F243*G243/100,F243*G243)","v":{"v":0,"d":"0.00"}}]
[]
[20911,"6.2.2.6",null,"400mm, beam (internal)","m²",{"v":16,"d":"16.0"},{"v":0,"d":"0.00"},{"$f":"IF(E245 = CHAR(37), F245*G245/100,F245*G245)","v":{"v":0,"d":"0.00"}}]
[]
[20912,"6.2.2.7",null,"Columns (290mm x 290mm x 1000mm)","No.",{"v":12,"d":"12.0"},{"v":0,"d":"0.00"},{"$f":"IF(E247 = CHAR(37), F247*G247/100,F247*G247)","v":{"v":0,"d":"0.00"}}]
[]
[20982,null,"8.2.2, PSG 8.2.2","Horizontal plane to"]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H208:H250)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 6 - ADMINISTRATION BUILDING EXTENSION"]
[{"$nulls":7},"SECTION 6.2: CONCRETE, FORMWORK AND REINFORCING"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H251","v":{"v":0,"d":"0.00"}}]
[20983,"6.2.2.8",null,"Roof slab soffit","m²",{"v":166,"d":"166.0"},{"v":0,"d":"0.00"},{"$f":"IF(E256 = CHAR(37), F256*G256/100,F256*G256)","v":{"v":0,"d":"0.00"}}]
[]
[20984,"6.2.2.9",null,"Floor slab soffit","m²",{"v":114,"d":"114.0"},{"v":0,"d":"0.00"},{"$f":"IF(E258 = CHAR(37), F258*G258/100,F258*G258)","v":{"v":0,"d":"0.00"}}]
[]
[20985,"6.2.2.10",null,"New walkway ","m²",{"v":50,"d":"50.0"},{"v":0,"d":"0.00"},{"$f":"IF(E260 = CHAR(37), F260*G260/100,F260*G260)","v":{"v":0,"d":"0.00"}}]
[]
[20987,null,null,"Narrow widths up to 300mm for smooth finish from formwork on"]
[]
[20988,null,"8.2.5","Vertical plane to"]
[]
[20989,"6.2.2.11",null,"Up to 200mm for concrete roof slab (including drip mould)","m",{"v":59,"d":"59.0"},{"v":0,"d":"0.00"},{"$f":"IF(E266 = CHAR(37), F266*G266/100,F266*G266)","v":{"v":0,"d":"0.00"}}]
[]
[21085,"6.2.2.12",null,"Up to 260mm for floor slab","m",{"v":59,"d":"59.0"},{"v":0,"d":"0.00"},{"$f":"IF(E268 = CHAR(37), F268*G268/100,F268*G268)","v":{"v":0,"d":"0.00"}}]
[]
[21086,"6.2.2.13",null,"Up to 200mm for walkway","m",{"v":59,"d":"59.0"},{"v":0,"d":"0.00"},{"$f":"IF(E270 = CHAR(37), F270*G270/100,F270*G270)","v":{"v":0,"d":"0.00"}}]
[]
[22463,"6.2.2.14",null,"Up to 100mm step up in floor slab","m",{"v":49,"d":"49.00"},{"v":0,"d":"0.00"},{"$f":"IF(E272 = CHAR(37), F272*G272/100,F272*G272)","v":{"v":0,"d":"0.00"}}]
[]
[21087,null,"8.2.5","Horizontal plane to"]
[]
[21088,"6.2.2.15",null,"290mm wide, beam ","m",{"v":45,"d":"45.0"},{"v":0,"d":"0.00"},{"$f":"IF(E276 = CHAR(37), F276*G276/100,F276*G276)","v":{"v":0,"d":"0.00"}}]
[]
[21090,"6.2.3","8.4.4\r\nPSG 5.2.1","UNFORMED SURFACE FINISHES"]
[]
[21091,null,"8.4.4 b)","Steel-float finish to slabs"]
[]
[21161,"6.2.3.1",null,"Roof slab","m²",{"v":166,"d":"166.0"},{"v":0,"d":"0.00"},{"$f":"IF(E282 = CHAR(37), F282*G282/100,F282*G282)","v":{"v":0,"d":"0.00"}}]
[]
[21092,"6.2.3.2",null,"Walkway slab","m²",{"v":48,"d":"48.0"},{"v":0,"d":"0.00"},{"$f":"IF(E284 = CHAR(37), F284*G284/100,F284*G284)","v":{"v":0,"d":"0.00"}}]
[]
[21093,"6.2.3.3",null,"Floor slab","m²",{"v":114,"d":"114.0"},{"v":0,"d":"0.00"},{"$f":"IF(E286 = CHAR(37), F286*G286/100,F286*G286)","v":{"v":0,"d":"0.00"}}]
[]
[20990,"6.2.4","8.5, 5.5.7, PSG 5.5.7","JOINTS"]
[]
[20991,"6.2.4.1",null,"Expansion joints with 10mm polystyrene between concrete roof slab and brick wall surfaces","m",{"v":100,"d":"100.0"},{"v":0,"d":"0.00"},{"$f":"IF(E290 = CHAR(37), F290*G290/100,F290*G290)","v":{"v":0,"d":"0.00"}}]
[]
[21107,"6.2.4.2",null,"Expansion joints with 10mm polystyrene between concrete floor slab and concrete walkway slab","m",{"v":50,"d":"50.0"},{"v":0,"d":"0.00"},{"$f":"IF(E292 = CHAR(37), F292*G292/100,F292*G292)","v":{"v":0,"d":"0.00"}}]
[]
[20992,"6.2.4.3",null,"Expansion joints with 10mm polystyrene between existing concrete roof slab and proposed concrete roof slab","m",{"v":12,"d":"12.0"},{"v":0,"d":"0.00"},{"$f":"IF(E294 = CHAR(37), F294*G294/100,F294*G294)","v":{"v":0,"d":"0.00"}}]
[]
[20993,"6.2.5","8.3, PSG 8.1.2","REINFORCEMENT"]
[]
[20994,null,"8.3.1","Mild steel reinforcement to structural concrete work"]
[]
[20995,"6.2.5.1",null,"Various diameter bars","t",1.1,{"v":0,"d":"0.00"},{"$f":"IF(E300 = CHAR(37), F300*G300/100,F300*G300)","v":{"v":0,"d":"0.00"}}]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H255:H301)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 6 - ADMINISTRATION BUILDING EXTENSION"]
[{"$nulls":7},"SECTION 6.2: CONCRETE, FORMWORK AND REINFORCING"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H302","v":{"v":0,"d":"0.00"}}]
[20996,null,"8.3.1","High tensile steel reinforcement to structural concrete work"]
[]
[20997,"6.2.5.2",null,"Various diameter bars","t",11.4,{"v":0,"d":"0.00"},{"$f":"IF(E309 = CHAR(37), F309*G309/100,F309*G309)","v":{"v":0,"d":"0.00"}}]
[]
[20998,null,"8.3.2","High tensile welded mesh reinforcement"]
[]
[21160,"6.2.5.3",null,"Mesh Ref 500","m²",{"v":50,"d":"50.0"},{"v":0,"d":"0.00"},{"$f":"IF(E313 = CHAR(37), F313*G313/100,F313*G313)","v":{"v":0,"d":"0.00"}}]
[]
[21108,"6.2.5.4",null,"Mesh Ref 395","m²",{"v":50,"d":"50.0"},{"v":0,"d":"0.00"},{"$f":"IF(E315 = CHAR(37), F315*G315/100,F315*G315)","v":{"v":0,"d":"0.00"}}]
[]
[21156,"6.2.6","PSG 5.5.8, PSG 8.4.7","CURING AND PROTECTION"]
[]
[21157,"6.2.6.1",null,"Floor slabs","m²",{"v":114,"d":"114.0"},{"v":0,"d":"0.00"},{"$f":"IF(E319 = CHAR(37), F319*G319/100,F319*G319)","v":{"v":0,"d":"0.00"}}]
[]
[21158,"6.2.6.2",null,"Wall Beams","m²",{"v":11,"d":"11.0"},{"v":0,"d":"0.00"},{"$f":"IF(E321 = CHAR(37), F321*G321/100,F321*G321)","v":{"v":0,"d":"0.00"}}]
[]
[21219,"6.2.6.3",null,"Roof slab","m²",{"v":166,"d":"166.0"},{"v":0,"d":"0.00"},{"$f":"IF(E323 = CHAR(37), F323*G323/100,F323*G323)","v":{"v":0,"d":"0.00"}}]
[]
[21220,"6.2.6.4",null,"New Walkway","m²",{"v":48,"d":"48.0"},{"v":0,"d":"0.00"},{"$f":"IF(E325 = CHAR(37), F325*G325/100,F325*G325)","v":{"v":0,"d":"0.00"}}]
[]
[21221,"6.2.6.5",null,"Floor Beam","m²",{"v":17,"d":"17.0"},{"v":0,"d":"0.00"},{"$f":"IF(E327 = CHAR(37), F327*G327/100,F327*G327)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":34}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H306:H361)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 6 - ADMINISTRATION BUILDING EXTENSION"]
[{"$nulls":7},"SECTION 6.3: MASONRY"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[20955,"6.3",null,"MASONRY"]
[]
[20999,null,null,"SUPPLEMENTARY PREAMBLES:"]
[]
[21000,null,null,"Sizes in descriptions"]
[]
[21001,null,null,"Where sizes in descriptions are given in brick units, 'one brick' shall represent the length and 'half brick' the width of a brick."]
[]
[21002,null,null,"Hollow walls, etc"]
[]
[21003,null,null,"Descriptions of hollow walls shall be deemed to include leaving every fifth perpend of the bottom course of the external skin open as a weep hole."]
[]
[21004,null,null,"Walls in two skins described as 'bagged and sealed' shall be deemed to include having the outer face of the inner skin bagged with 1:6 cement and sand mixture"]
[]
[21005,null,null,"Face bricks"]
[]
[21006,null,null,"Bricks shall be ordered timeously to obtain uniformity in size and colour"]
[]
[21007,null,null,"Pointing"]
[]
[21008,null,null,"Descriptions of recessed pointing to fair face brickwork and face brickwork shall be deemed to include square recessed, hollow recessed, weathered pointing, etc."]
[]
[21009,"6.3.1","PABR","BRICKWORK IN SUPERSTRUCTURE"]
[]
[21192,null,null,"In mortar class according to PABR 2.6:"]
[]
[21010,null,null,"Existing Building"]
[]
[21011,null,null,"New internal walls in common NFP brick to be plastered and painted (measured elsewhere)"]
[]
[21012,"6.3.1.1",null,"Single skin wall","m²",{"v":15,"d":"15.0"},{"v":0,"d":"0.00"},{"$f":"IF(E396 = CHAR(37), F396*G396/100,F396*G396)","v":{"v":0,"d":"0.00"}}]
[]
[21013,null,null,"Proposed Administration Building"]
[]
[21014,null,null,"New external one brick walls in Roan Satin FBX facebrick skin externally with common NFP brick skin internally to be plastered and painted (measured elsewhere)"]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H366:H400)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 6 - ADMINISTRATION BUILDING EXTENSION"]
[{"$nulls":7},"SECTION 6.3: MASONRY"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H401","v":{"v":0,"d":"0.00"}}]
[21096,"6.3.1.2",null,"External facebrick skin ","m²",{"v":128,"d":"128.0"},{"v":0,"d":"0.00"},{"$f":"IF(E406 = CHAR(37), F406*G406/100,F406*G406)","v":{"v":0,"d":"0.00"}}]
[]
[21097,"6.3.1.3",null,"Internal common brick skin ","m²",{"v":128,"d":"128.0"},{"v":0,"d":"0.00"},{"$f":"IF(E408 = CHAR(37), F408*G408/100,F408*G408)","v":{"v":0,"d":"0.00"}}]
[]
[21098,null,null,"New internal walls in common NFP brickwork to be plastered and painted (measured elsewhere)"]
[]
[21099,"6.3.1.4",null,"Single skin wall ","m²",{"v":50,"d":"50.0"},{"v":0,"d":"0.00"},{"$f":"IF(E412 = CHAR(37), F412*G412/100,F412*G412)","v":{"v":0,"d":"0.00"}}]
[]
[21100,"6.3.1.5",null,"Double skin wall ","m²",{"v":30,"d":"30.0"},{"v":0,"d":"0.00"},{"$f":"IF(E414 = CHAR(37), F414*G414/100,F414*G414)","v":{"v":0,"d":"0.00"}}]
[]
[21015,"6.3.2","PABR","BRICKWORK SUNDRIES"]
[]
[21016,null,null,"Brick on edge lintels"]
[]
[21017,"6.3.2.1",null,"110 x 150mm lintels in lengths not exceeding 3m","m",{"v":20,"d":"20.0"},{"v":0,"d":"0.00"},{"$f":"IF(E420 = CHAR(37), F420*G420/100,F420*G420)","v":{"v":0,"d":"0.00"}}]
[]
[21018,null,null,"Brick on edge sills"]
[]
[21019,"6.3.2.2",null,"110 x 150mm sills in lengths not exceeding 3m","m",{"v":26,"d":"26.0"},{"v":0,"d":"0.00"},{"$f":"IF(E424 = CHAR(37), F424*G424/100,F424*G424)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":35}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H405:H459)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 6 - ADMINISTRATION BUILDING EXTENSION"]
[{"$nulls":7},"SECTION 6.4: WATERPROOFING"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[20956,"6.4",null,"WATERPROOFING"]
[]
[21020,null,null,"SUPPLEMENTARY PREAMBLES:"]
[]
[21021,null,null,"Waterproofing"]
[]
[21022,null,null,"Waterproofing of roofs, etc shall be laid under a ten year guarantee. Waterproofing to roofs shall be laid to even falls to outlets etc with necessary ridges, hips and valleys. Descriptions of sheet or membrane waterproofing shall be deemed to include additional labour to turn-ups and turn-downs"]
[]
[21023,"6.4.1",null,"DAMP PROOFING OF ROOF"]
[]
[21024,null,null,"One layer of Derbigum SP (Special Polyester) waterproof sheeting sealed "]
[]
[21025,"6.4.1.1",null,"Top of Concrete Roof","m²",{"v":166,"d":"166.0"},{"v":0,"d":"0.00"},{"$f":"IF(E476 = CHAR(37), F476*G476/100,F476*G476)","v":{"v":0,"d":"0.00"}}]
[]
[21190,null,null,"One primer coat and one slurry coat Cemflex or similar approved coating, including water and portland cement for mix"]
[]
[21191,"6.4.1.2",null,"In shower walls and floors","m²",{"v":80,"d":"80.0"},{"v":0,"d":"0.00"},{"$f":"IF(E480 = CHAR(37), F480*G480/100,F480*G480)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":30}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H464:H510)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 6 - ADMINISTRATION BUILDING EXTENSION"]
[{"$nulls":7},"SECTION 6.5: METALWORK"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[20957,"6.5","SANS 1200 H, PSHA, PACP","METALWORK"]
[]
[21026,"6.5.1",null,"SUPPLEMENTARY PREAMBLES"]
[]
[21027,null,null,"The following to be finished with 25 microns powder coated, manufactured and installed in accordance with good building practice and in terms of the latest code of practice with revisions as recommended by SANS and AAAMSA"]
[]
[21028,null,null,"Items shall be manufactured by an approved specialist who shall provide a sample upon request, for the Engineers approval"]
[]
[21029,null,null,"Tenderers are advised to refer to the Architect's window and door schedules attached to these Bills of Quantities for details on drawing 030"]
[]
[21030,null,null,"Tenderers are to note that should there be any doubt or obscurity as to the meaning and intent of any descriptions, the Contractor must have the same rectified and allow for same accordingly in his tender. The Contractor is to include in his rates for all that he considers necessary for the proper construction of the windows and doors. No claims whatsoever will be afterwards admitted due to the Contractor having failed to comply with these conditions"]
[]
[21031,null,null,"Rates shall include for the following:"]
[]
[21032,null,null,"1. All opening and fixed lights, coupling mullions and transoms, support steelwork, fittings, ironmongery, etc., as required and specified."]
[]
[21033,null,null,"2. Complete glazing as described, with and including matching aluminium glazing beads and gaskets and glazed in accordance with the manufacturer's written instructions"]
[]
[]
[]
[]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H515:H536)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 6 - ADMINISTRATION BUILDING EXTENSION"]
[{"$nulls":7},"SECTION 6.5: METALWORK"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H537","v":{"v":0,"d":"0.00"}}]
[21034,null,null,"3. Building in and fixing into preformed openings. Window opening sizes to be verified on site before windows can be manufactured"]
[]
[21035,null,null,"4. Suitably protecting all exposed aluminium and glass surfaces with an approved protection tape and plastic sheeting. Such protection is to be removed at completion of the contract and the exposed surfaces cleaned down and left perfect. Under no circumstances will any damage whatsoever to the finished product be acceptable"]
[]
[21036,null,null,"5. Silicone pointing with a silicone sealant recommended by AAAMSA on all door / window and structure junctions"]
[]
[21037,"6.5.2",null,"NATURAL ANODISED ALUMINIUM WINDOWS, DOORS, ETC."]
[]
[21105,null,null,"Note: Tenderers are to refer to the Architects door schedules when pricing the items hereunder"]
[]
[21038,null,null,"Hardwood Meranti door frames plugged to brickwork "]
[]
[21039,"6.5.2.1",null,"WD01","No.",{"v":10,"d":"10.0"},{"v":0,"d":"0.00"},{"$f":"IF(E554 = CHAR(37), F554*G554/100,F554*G554)","v":{"v":0,"d":"0.00"}}]
[]
[21040,null,null,"Note: Tenderers are to refer to the attached Architects window schedules when pricing the items hereunder"]
[]
[21041,null,null,"Wispeco/similar standard aluminium window frame plugged to brickwork or concrete, complete with burglar bars"]
[]
[21042,"6.5.2.2",null,"AW01","No.",{"v":8,"d":"8.0"},{"v":0,"d":"0.00"},{"$f":"IF(E560 = CHAR(37), F560*G560/100,F560*G560)","v":{"v":0,"d":"0.00"}}]
[]
[21101,"6.5.2.3",null,"AW02","No.",{"v":14,"d":"14.0"},{"v":0,"d":"0.00"},{"$f":"IF(E562 = CHAR(37), F562*G562/100,F562*G562)","v":{"v":0,"d":"0.00"}}]
[]
[21193,null,null,"Tinted glass"]
[]
[21194,"6.5.2.4",null,"Allow for all external glass windows and doors to be tinted with 20%, 2-ply, non-reflective film","Sum",{"v":1,"d":"1.0"},{"v":0,"d":"0.00"},{"$f":"IF(E566 = CHAR(37), F566*G566/100,F566*G566)","v":{"v":0,"d":"0.00"}}]
[]
[21195,"6.5.2.5",null,"Allow for glass awareness decals on all doors","Sum",{"v":1,"d":"1.0"},{"v":0,"d":"0.00"},{"$f":"IF(E568 = CHAR(37), F568*G568/100,F568*G568)","v":{"v":0,"d":"0.00"}}]
[]
[21043,"6.5.3",null,"SHOWER CUBICLE DOORS"]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H541:H570)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 6 - ADMINISTRATION BUILDING EXTENSION"]
[{"$nulls":7},"SECTION 6.5: METALWORK"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H571","v":{"v":0,"d":"0.00"}}]
[21044,null,null,"KAL or equal approved classic pivot shower door, in natural anodised finish including frames, all fixed complete to walls including pointing with clear silicone all round both sides of frame"]
[]
[21045,"6.5.3.1",null,"Swing door, 900mm wide x 2,032mm high","No.",{"v":4,"d":"4.0"},{"v":0,"d":"0.00"},{"$f":"IF(E578 = CHAR(37), F578*G578/100,F578*G578)","v":{"v":0,"d":"0.00"}}]
[]
[21106,"6.5.4","SANS 1200 H\r\nPSHA","STRUCTURAL STEEL"]
[]
[21150,null,"8.3.7","HANDRAILS"]
[]
[21222,"6.5.4.1",null,"Removal of the existing handrails","m",{"v":80,"d":"80.0"},{"v":0,"d":"0.00"},{"$f":"IF(E584 = CHAR(37), F584*G584/100,F584*G584)","v":{"v":0,"d":"0.00"}}]
[]
[21151,null,"8.3.7 b)","Supply and install stainless steel handrail assembly complete with stanchions, bends and ends with chemical anchors"]
[]
[21152,"6.5.4.2","8.3.7 b) 1)","Horizontal (hand and knee rails)","m",{"v":80,"d":"80.0"},{"v":0,"d":"0.00"},{"$f":"IF(E588 = CHAR(37), F588*G588/100,F588*G588)","v":{"v":0,"d":"0.00"}}]
[]
[21153,"6.5.4.3","8.3.7 b) 2)","Sloping","m",{"v":10,"d":"10.0"},{"v":0,"d":"0.00"},{"$f":"IF(E590 = CHAR(37), F590*G590/100,F590*G590)","v":{"v":0,"d":"0.00"}}]
[]
[21154,"6.5.4.4","8.3.7 b) 3)","Shaped ends and bends","No.",{"v":8,"d":"8.0"},{"v":0,"d":"0.00"},{"$f":"IF(E592 = CHAR(37), F592*G592/100,F592*G592)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":30}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H575:H622)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 6 - ADMINISTRATION BUILDING EXTENSION"]
[{"$nulls":7},"SECTION 6.6: PLASTERING"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[20958,"6.6","PABR 5.3.1\r\nPABR 2.1\r\n","PLASTERING"]
[]
[21046,"6.6.1",null,"PRICES"]
[]
[21047,null,null,"The prices of mouldings, weathering, skirting, labours, etc. shall include for forming mitres, stops, etc. unless otherwise described"]
[]
[21048,null,null,"The prices of all rendering shall include for working around pipes, balusters, etc"]
[]
[21049,null,null,"Rates for plaster are to include for all filling to and working around electrical conduits, etc., prior to plastering"]
[]
[21050,"6.6.2",null,"SCREEDS"]
[]
[21051,null,null,"Screeds steel trowelled to falls, on concrete"]
[]
[21052,"6.6.2.1",null,"1:3 cement plaster, 30mm min thick on floors and landings","m²",{"v":315,"d":"315.0"},{"v":0,"d":"0.00"},{"$f":"IF(E641 = CHAR(37), F641*G641/100,F641*G641)","v":{"v":0,"d":"0.00"}}]
[]
[21053,"6.6.3",null,"INTERNAL PLASTER"]
[]
[21054,null,null,"One coat cement plaster on brickwork:"]
[]
[21055,"6.6.3.1",null,"Walls","m²",{"v":500,"d":"500.0"},{"v":0,"d":"0.00"},{"$f":"IF(E647 = CHAR(37), F647*G647/100,F647*G647)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":25}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H627:H672)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 6 - ADMINISTRATION BUILDING EXTENSION"]
[{"$nulls":7},"SECTION 6.7: TILING"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[20959,"6.7",null,"TILING"]
[]
[21056,"6.7.1",null,"SUPPLEMENTARY PREAMBLES"]
[]
[21057,null,null,"Rates for tiling must include for fixing, adhesive, anti-bacteria grout, sealing, wastage, profit, etc"]
[]
[21058,"6.7.2",null,"WALL TILING, ETC"]
[]
[21059,null,null,"Supply and fix tiles to match existing with supplier specified tile adhesive, applied with notched trowel, with flush pointed anti-bacteria 2mm grouting"]
[]
[21196,null,null,"1. Materials (nett area) - R250 PC amount of R/m²"]
[]
[21197,null,null,"2. Proportion of rate adjustable related to PC amount (e.g.: waste, etc.) - R"]
[]
[21198,null,null,"3. Proportion of rate not adjustable (e.g.: labour, etc.) - R"]
[]
[21060,"6.7.2.1",null,"On walls (value to rate column)","m²",{"v":300,"d":"300.0"},{"v":0,"d":"0.00"},{"$f":"IF(E693 = CHAR(37), F693*G693/100,F693*G693)","v":{"v":0,"d":"0.00"}}]
[]
[21061,"6.7.3",null,"FLOOR TILING, ETC"]
[]
[21062,null,null,"Supply and fix tiles to match existing with supplier specified tile adhesive, applied with notched trowel, with flush pointed anti-bacteria 4mm grouting"]
[]
[21199,null,null,"1. Materials (nett area) - R250 PC amount of R/m²"]
[]
[21200,null,null,"2. Proportion of rate adjustable related to PC amount (e.g.: waste, etc.) - R"]
[]
[21201,null,null,"3. Proportion of rate not adjustable (e.g.: labour, etc.) - R"]
[]
[21063,"6.7.3.1",null,"On floors","m²",{"v":152,"d":"152.0"},{"v":0,"d":"0.00"},{"$f":"IF(E705 = CHAR(37), F705*G705/100,F705*G705)","v":{"v":0,"d":"0.00"}}]
[]
[21064,"6.7.4",null,"SKIRTING, NOSING, ETC"]
[]
[21202,null,null,"1. Materials (nett area) - R250 PC amount of R/m²"]
[]
[21203,null,null,"2. Proportion of rate adjustable related to PC amount (e.g.: waste, etc.) - R"]
[]
[21204,null,null,"3. Proportion of rate not adjustable (e.g.: labour, etc.) - R"]
[]
[21065,"6.7.4.1",null,"Tile skirting to match existing","m",{"v":200,"d":"200.0"},{"v":0,"d":"0.00"},{"$f":"IF(E715 = CHAR(37), F715*G715/100,F715*G715)","v":{"v":0,"d":"0.00"}}]
[]
[21102,"6.7.5",null,"POLISH, SEALER, ETC"]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H677:H717)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 6 - ADMINISTRATION BUILDING EXTENSION"]
[{"$nulls":7},"SECTION 6.7: TILING"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H718","v":{"v":0,"d":"0.00"}}]
[21103,"6.7.5.1",null,"Two coats approved sealer on tile flooring","m²",{"v":152,"d":"152.0"},{"v":0,"d":"0.00"},{"$f":"IF(E723 = CHAR(37), F723*G723/100,F723*G723)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":56}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H722:H779)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 6 - ADMINISTRATION BUILDING EXTENSION"]
[{"$nulls":7},"SECTION 6.8: PAINTING"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[20960,"6.8",null,"PAINTING"]
[]
[21066,"6.8.1",null,"PREPARATORY WORK TO EXISTING WORK"]
[]
[21067,null,null,"Previously painted plastered surfaces:"]
[]
[21068,null,null,"Surfaces shall be thoroughly washed down and allowed to dry completely before any paint is applied. Blistered or peeling paint shall be completely removed and cracks shall be opened, filled with a suitable filler and finished smooth"]
[]
[21069,null,null,"Previously painted metal surfaces:"]
[]
[21070,null,null,"Surfaces shall be thoroughly rubbed and cleaned down. Blistered or peeling paint shall be completely removed down to bare metal"]
[]
[21071,null,null,"Previously painted wood surfaces:"]
[]
[21072,null,null,"Surfaces shall be thoroughly cleaned down. Blistered or peeling paint shall be completely removed and cracks and crevices shall be primed, filled with suitable filler and finished smooth"]
[]
[21073,"6.8.2",null,"PAINTWORK ETC TO PREVIOUSLY PAINTED WORK ON FLOATED PLASTER"]
[]
[21074,null,null,"Prepare and brush surface to remove all loose contaminants and apply and two coats interior quality acrylic emulsion paint"]
[]
[21075,"6.8.2.1",null,"On existing internal walls","m²",{"v":225,"d":"225.0"},{"v":0,"d":"0.00"},{"$f":"IF(E804 = CHAR(37), F804*G804/100,F804*G804)","v":{"v":0,"d":"0.00"}}]
[]
[21077,"6.8.3",null,"PAINTWORK, ETC. TO NEW WORK ON INTERNAL FLOATED PLASTERED SURFACES"]
[]
[21078,null,null,"One coat plaster primer, one undercoat and two finishing coats non drip enamel for interior application"]
[]
[21079,"6.8.3.1",null,"On internal Walls","m²",{"v":245,"d":"245.0"},{"v":0,"d":"0.00"},{"$f":"IF(E810 = CHAR(37), F810*G810/100,F810*G810)","v":{"v":0,"d":"0.00"}}]
[]
[21205,"6.8.4",null,"PAINTWORK, ETC. TO NEW WORK ON INTERNAL CEILING SURFACES"]
[]
[]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H784:H815)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 6 - ADMINISTRATION BUILDING EXTENSION"]
[{"$nulls":7},"SECTION 6.8: PAINTING"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H816","v":{"v":0,"d":"0.00"}}]
[21206,null,null,"One coat plaster primer, one undercoat and two finishing coats non drip enamel for interior application"]
[]
[22464,"6.8.4.1",null,"On ceiling of existing and new buildings","m²",{"v":152,"d":"152.00"},{"v":0,"d":"0.00"},{"$f":"IF(E823 = CHAR(37), F823*G823/100,F823*G823)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":51}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H820:H874)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 6 - ADMINISTRATION BUILDING EXTENSION"]
[{"$nulls":7},"SECTION 6.9: SEWER"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[21166,"6.9","SANS1200 LD, PSLD","SEWER"]
[]
[22465,null,null,"Ablution & Changeroom Facilities (Male & Female) & New Admin Building"]
[]
[22466,"6.9.1",null,"Supply and install associated sewer pipework and fittings for the sewer to the new Administration building, including modifications, new pipework/fittings and replacement of pipework and fittings to the Ablution and Changeroom facilities","Prov Sum",{"v":1,"d":"1.00"},{"v":20000,"d":"20,000.00"},{"v":20000,"d":"20,000.00"}]
[]
[22467,"6.9.2",null,"Overheads, charges and profit on above item 6.9.1","%",{"$f":"H883","v":{"v":20000,"d":"20,000.00"}},{"v":0,"d":"0.00"},{"$f":"IF(E885 = CHAR(37), F885*G885/100,F885*G885)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":43}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H879:H928)","v":{"v":20000,"d":"20,000.00"}}]
[null,"SCHEDULE 6 - ADMINISTRATION BUILDING EXTENSION"]
[{"$nulls":7},"SECTION 6.10: WATER SUPPLY"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[22444,"6.10",null,"GENERAL ITEMS"]
[]
[22475,null,null,"Ablution & Changeroom Facilities (Male & Female) & New Admin Building"]
[]
[22476,"6.10.1",null,"Supply and install associated pipework, valves and fittings for the water supply to the new Administration building, including modifications, new pipework/fittings and replacement of pipework, valves and fittings to the Ablution and Changeroom facilities","Prov Sum",{"v":1,"d":"1.00"},{"v":25000,"d":"25,000.00"},{"v":25000,"d":"25,000.00"}]
[]
[22477,"6.10.2",null,"Overheads, charges and profit on above item 6.10.1","%",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"$f":"IF(E939 = CHAR(37), F939*G939/100,F939*G939)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":43}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H933:H982)","v":{"v":25000,"d":"25,000.00"}}]
[null,"SCHEDULE 6 - ADMINISTRATION BUILDING EXTENSION"]
[{"$nulls":7},"SECTION 6.11: PROVISIONAL SUMS"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[21110,"6.11",null,"PROVISIONAL SUMS"]
[]
[21111,null,null,"Signage"]
[]
[21112,"6.11.1",null,"Supply and install signage ","Prov Sum",{"v":1,"d":"1.0"},{"v":10000,"d":"10,000.00"},{"v":10000,"d":"10,000.00"}]
[]
[21113,"6.11.2",null,"Overheads, charges and profit on above item 6.11.1","%",{"$f":"H991","v":{"v":10000,"d":"10,000.0"}},{"v":0,"d":"0.00"},{"$f":"IF(E993 = CHAR(37), F993*G993/100,F993*G993)","v":{"v":0,"d":"0.00"}}]
[]
[21114,null,null,"Ablution & Changeroom Facilities (Male & Female) & Laboratory"]
[]
[21115,"6.11.3",null,"Supply and install wash hand basins and sinks","Prov Sum",{"v":1,"d":"1.0"},{"v":20000,"d":"20,000.00"},{"v":20000,"d":"20,000.00"}]
[]
[21116,"6.11.4",null,"Overheads, charges and profit on above item 6.11.3","%",{"$f":"H997","v":{"v":20000,"d":"20,000.0"}},{"v":0,"d":"0.00"},{"$f":"IF(E999 = CHAR(37), F999*G999/100,F999*G999)","v":{"v":0,"d":"0.00"}}]
[]
[21117,null,null,"Ablution & Changeroom Facilities (Male & Female)"]
[]
[21118,"6.11.5",null,"Supply and install toilets","Prov Sum",{"v":1,"d":"1.0"},{"v":20000,"d":"20,000.00"},{"v":20000,"d":"20,000.00"}]
[]
[21119,"6.11.6",null,"Overheads, charges and profit on above item 6.11.5","%",{"$f":"H1003","v":{"v":20000,"d":"20,000.0"}},{"v":0,"d":"0.00"},{"$f":"IF(E1005 = CHAR(37), F1005*G1005/100,F1005*G1005)","v":{"v":0,"d":"0.00"}}]
[]
[21120,null,null,"Ablution & Changeroom Facilities (Male & Female)"]
[]
[21121,"6.11.7",null,"Supply and install showers (hot and cold water)","Prov Sum",{"v":1,"d":"1.0"},{"v":25000,"d":"25,000.00"},{"v":25000,"d":"25,000.00"}]
[]
[21122,"6.11.8",null,"Overheads, charges and profit on above item 6.11.7","%",{"$f":"H1009","v":{"v":25000,"d":"25,000.0"}},{"v":0,"d":"0.00"},{"$f":"IF(E1011 = CHAR(37), F1011*G1011/100,F1011*G1011)","v":{"v":0,"d":"0.00"}}]
[]
[21213,null,"C5.2.6","Network Installation"]
[]
[21214,"6.11.9",null,"Supply and install fibre or equivalent network connection to the site","Prov Sum",{"v":1,"d":"1.0"},{"v":50000,"d":"50,000.00"},{"v":50000,"d":"50,000.00"}]
[]
[21215,"6.11.10",null,"Overheads, charges and profit on above item 6.11.9","%",{"$f":"H1015","v":{"v":50000,"d":"50,000.0"}},{"v":0,"d":"0.00"},{"$f":"IF(E1017 = CHAR(37), F1017*G1017/100,F1017*G1017)","v":{"v":0,"d":"0.00"}}]
[]
[21147,null,"PS9.13.4","Fire reticulation, Fire Services, Fire Supplies and Fire Signage"]
[]
[21148,"6.11.11",null,"Supply and install all fire reticulation, fire services, fire supplies and fire signage","Prov Sum",{"v":1,"d":"1.0"},{"v":35000,"d":"35,000.00"},{"v":35000,"d":"35,000.00"}]
[]
[21149,"6.11.12",null,"Overheads, charges and profit on above item 6.11.11","%",{"$f":"H1021","v":{"v":35000,"d":"35,000.0"}},{"v":0,"d":"0.00"},{"$f":"IF(E1023 = CHAR(37), F1023*G1023/100,F1023*G1023)","v":{"v":0,"d":"0.00"}}]
[]
[21186,null,null,"Furniture for offices, labs, boardrooms, workshop, control room, and kitchen"]
[]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H987:H1027)","v":{"v":160000,"d":"160,000.00"}}]
[null,"SCHEDULE 6 - ADMINISTRATION BUILDING EXTENSION"]
[{"$nulls":7},"SECTION 6.11: PROVISIONAL SUMS"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H1028","v":{"v":160000,"d":"160,000.00"}}]
[21187,"6.11.13",null,"Supply and install furniture for offices, labs, boardrooms, workshop, control room, and kitchen","Prov Sum",{"v":1,"d":"1.0"},{"v":200000,"d":"200,000.00"},{"v":200000,"d":"200,000.00"}]
[]
[21188,"6.11.14",null,"Overheads, charges and profit on above item 6.11.13","%",{"$f":"H1033","v":{"v":200000,"d":"200,000.0"}},{"v":0,"d":"0.00"},{"$f":"IF(E1035 = CHAR(37), F1035*G1035/100,F1035*G1035)","v":{"v":0,"d":"0.00"}}]
[]
[23071,null,null,"Associated stormwater works including pipework and fittings etc."]
[]
[23072,"6.11.15",null,"Supply and install associated stormwater works","Prov Sum",{"v":1,"d":"1.00"},{"v":25000,"d":"25,000.00"},{"v":25000,"d":"25,000.00"}]
[]
[23073,"6.11.16",null,"Overheads, charges and profit on above item 6.11.15","%",{"$f":"H1039","v":{"v":25000,"d":"25,000.00"}},{"v":0,"d":"0.00"},{"$f":"IF(E1041 = CHAR(37), F1041*G1041/100,F1041*G1041)","v":{"v":0,"d":"0.00"}}]
[]
[23081,null,null,"Ancillary items"]
[]
[23074,"6.11.17",null,"Supply and install ancillary items","Prov Sum",{"v":1,"d":"1.00"},{"v":50000,"d":"50,000.00"},{"v":50000,"d":"50,000.00"}]
[]
[23075,"6.11.18",null,"Overheads, charges and profit on above item 6.11.17","%",{"$f":"H1045","v":{"v":50000,"d":"50,000.00"}},{"v":0,"d":"0.00"},{"$f":"IF(E1047 = CHAR(37), F1047*G1047/100,F1047*G1047)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":35}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H1032:H1082)","v":{"v":435000,"d":"435,000.00"}}]
[null,"SCHEDULE 6 - ADMINISTRATION BUILDING EXTENSION"]
[{"$nulls":7},"SECTION 6.12: GENERAL"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[21162,"6.12",null,"GENERAL ITEMS"]
[]
[21167,"6.12.1",null,"Temporary Offices for EWS Operators"]
[]
[21174,"6.12.1.1",null,"Supply and maintenance of temporary on site airconditioned, insulated, furnished offices for the EWS Operators on site for the duration of the Contract (Including temporary ablution facilities)","Sum",{"v":1,"d":"1.0"},{"v":0,"d":"0.00"},{"$f":"IF(E1091 = CHAR(37), F1091*G1091/100,F1091*G1091)","v":{"v":0,"d":"0.00"}}]
[]
[21175,"6.12.2",null,"GENERAL"]
[]
[21176,null,null,"Any other item the tenderer considers has been omitted and which requires pricing as separate items."]
[]
[21163,"6.12.2.1",null,"i)","Sum",{"v":1,"d":"1.0"},{"v":0,"d":"0.00"},{"$f":"IF(E1097 = CHAR(37), F1097*G1097/100,F1097*G1097)","v":{"v":0,"d":"0.00"}}]
[]
[21164,"6.12.2.2",null,"ii)","Sum",{"v":1,"d":"1.0"},{"v":0,"d":"0.00"},{"$f":"IF(E1099 = CHAR(37), F1099*G1099/100,F1099*G1099)","v":{"v":0,"d":"0.00"}}]
[]
[21165,"6.12.2.3",null,"iii)","Sum",{"v":1,"d":"1.0"},{"v":0,"d":"0.00"},{"$f":"IF(E1101 = CHAR(37), F1101*G1101/100,F1101*G1101)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":38}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H1087:H1139)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 6 - ADMINISTRATION BUILDING EXTENSION"]
[{"$nulls":3},"SUMMARY OF SECTIONS"]
[null," ","SECTION","DESCRIPTION",{"$nulls":3},"AMOUNT\n(RAND)"]
[null,null,"6.1","SECTION 6.1: ALTERATIONS",{"$nulls":3},{"$f":"H178","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"6.2","SECTION 6.2: CONCRETE, FORMWORK AND REINFORCING",{"$nulls":3},{"$f":"H362","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"6.3","SECTION 6.3: MASONRY",{"$nulls":3},{"$f":"H460","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"6.4","SECTION 6.4: WATERPROOFING",{"$nulls":3},{"$f":"H511","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"6.5","SECTION 6.5: METALWORK",{"$nulls":3},{"$f":"H623","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"6.6","SECTION 6.6: PLASTERING",{"$nulls":3},{"$f":"H673","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"6.7","SECTION 6.7: TILING",{"$nulls":3},{"$f":"H780","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"6.8","SECTION 6.8: PAINTING",{"$nulls":3},{"$f":"H875","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"6.9","SECTION 6.9: SEWER",{"$nulls":3},{"$f":"H929","v":{"v":20000,"d":"20,000.00"}}]
[]
[null,null,"6.10","SECTION 6.10: WATER SUPPLY",{"$nulls":3},{"$f":"H983","v":{"v":25000,"d":"25,000.00"}}]
[]
[null,null,"6.11","SECTION 6.11: PROVISIONAL SUMS",{"$nulls":3},{"$f":"H1083","v":{"v":435000,"d":"435,000.00"}}]
[]
[null,null,"6.12","SECTION 6.12: GENERAL",{"$nulls":3},{"$f":"H1140","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":35}
[null,null," Total Carried Forward To Summary Of Schedules"," Total Carried Forward To Summary Of Schedules",{"$nulls":3},{"$f":"SUM(H1144:H1201)","v":{"v":480000,"d":"480,000.00"}}]

{"sheet":"Schedule 7","index":6,"n_rows":745,"n_cols":8,"rows_kept":745}
["Rate=G","SCHEDULE 7 - SECURITY GUARD HOUSE"]
[{"$nulls":7},"SECTION 7.1: SITE CLEARANCE"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[21670,"7.1","SANS 1200 C, PSC & PSDB","SITE CLEARANCE"]
[]
[21915,null,null,"All drawing references are prefixed with 60398/10"]
[]
[21671,"7.1.1",null,"SITE CLEARANCE"]
[]
[21672,null,"8.2.1, PSC 8.2.1","Clear and grub site"]
[]
[21747,"7.1.1.1","PSC 8.2.11","Saw Cutting of existing asphalt surfaces","m",{"v":15,"d":"15.0"},{"v":0,"d":"0.00"},{"$f":"IF(E12 = CHAR(37), F12*G12/100,F12*G12)","v":{"v":0,"d":"0.00"}}]
[]
[21920,"7.1.1.2","PSC8.2.13","Remove existing road asphalt and spoil at approved spoil disposal site for up to 60mm","m²",{"v":13,"d":"13.0"},{"v":0,"d":"0.00"},{"$f":"IF(E14 = CHAR(37), F14*G14/100,F14*G14)","v":{"v":0,"d":"0.00"}}]
[]
[21754,null,"8.2.4","Re-clear surfaces where directed by Engineer (Provisional)"]
[]
[21755,"7.1.1.3",null,"Guard House site","m²",{"v":15,"d":"15.0"},{"v":0,"d":"0.00"},{"$f":"IF(E18 = CHAR(37), F18*G18/100,F18*G18)","v":{"v":0,"d":"0.00"}}]
[]
[21838,"7.1.1.4","8.2.10 PSC 8.2.10","Remove topsoil to depth of 150mm and stockpile","m³",{"v":4,"d":"4.0"},{"v":0,"d":"0.00"},{"$f":"IF(E20 = CHAR(37), F20*G20/100,F20*G20)","v":{"v":0,"d":"0.00"}}]
[]
[21957,null,"8.2.7, PSC 8.2.7","Existing Services"]
[]
[21766,null,"8.2.8","Demolish and remove structures/buildings and dismantle steelwork"]
[]
[21839,"7.1.1.5",null,"Disconnect, dismantle as needed, and remove the guard hut.","No.",{"v":1,"d":"1.0"},{"v":0,"d":"0.00"},{"$f":"IF(E26 = CHAR(37), F26*G26/100,F26*G26)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":25}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H4:H51)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 7 - SECURITY GUARD HOUSE"]
[{"$nulls":7},"SECTION 7.2: EARTHWORKS"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[21673,"7.2","SANS 1200 D, PSD","EARTHWORKS"]
[]
[21719,"7.2.1","8.3.3, PSD 8.3.3(a), PSD 2.3","RESTRICTED EXCAVATION"]
[]
[21674,null,"8.3.3 a), PSD 8.3.5.2","Restricted excavation in all materials and stockpile suitable material and use for embankment or backfill, and dispose of unsuitable material to an approved spoil site to be determined by the contractor"]
[]
[21675,"7.2.1.1",null,"Strip Footing","m³",{"v":9,"d":"9.0"},{"v":0,"d":"0.00"},{"$f":"IF(E62 = CHAR(37), F62*G62/100,F62*G62)","v":{"v":0,"d":"0.00"}}]
[]
[21959,"7.2.1.2",null,"Septic Tank","m³",{"v":10,"d":"10.0"},{"v":0,"d":"0.00"},{"$f":"IF(E64 = CHAR(37), F64*G64/100,F64*G64)","v":{"v":0,"d":"0.00"}}]
[]
[21840,"7.2.2",null,"FOUNDATION PREPARATION"]
[]
[21720,"7.2.2.1",null,"Compact bottom of excavation of in-situ material to 95% MOD AASHTO including testing","m²",{"v":16,"d":"16.0"},{"v":0,"d":"0.00"},{"$f":"IF(E68 = CHAR(37), F68*G68/100,F68*G68)","v":{"v":0,"d":"0.00"}}]
[]
[21676,"7.2.3",null,"BACKFILL"]
[]
[21841,null,"PSD 8.3.4.1","Selected backfill or fill material obtained from stockpile"]
[]
[21842,"7.2.3.1",null,"Fill embankment compacted to 95% MOD AASHTO in 150mm layers including testing","m³",{"v":20,"d":"20.0"},{"v":0,"d":"0.00"},{"$f":"IF(E74 = CHAR(37), F74*G74/100,F74*G74)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":27}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H56:H101)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 7 - SECURITY GUARD HOUSE"]
[{"$nulls":7},"SECTION 7.3: EARTHWORKS (PIPE TRENCHES)"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[22566,"7.3","SABS1200 DB","EARTHWORKS (PIPE TRENCHES)"]
[]
[22567,"7.3.1","PSDB 5.2 \r\n8.3.2","EXCAVATION"]
[]
[22572,null,"8.3.2 (a) PSDB 8.3.2 (a)","Excavate in all materials for pipe trenches, backfill, compact to specification and dispose of surplus/unsuitable material, for pipes:"]
[]
[22573,null,null,"Up to DN200 pipeline for a total trench depth"]
[]
[22574,"7.3.1.1",null,"Up to 3.0m","m³",{"v":15,"d":"15.00"},{"v":0,"d":"0.00"},{"$f":"IF(E114 = CHAR(37), F114*G114/100,F114*G114)","v":{"v":0,"d":"0.00"}}]
[]
[22575,null,"8.3.2 (b) PSDB 8.3.2 (b)","Extra-over Item 7.3.1.1 for excavation in (All provisional):"]
[]
[22576,"7.3.1.2",null,"1) Intermediate excavation","m³",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E118 = CHAR(37), F118*G118/100,F118*G118)","v":{"v":0,"d":"0.00"}}]
[]
[22577,"7.3.1.3",null,"2) Hard rock excavation","m³",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E120 = CHAR(37), F120*G120/100,F120*G120)","v":{"v":0,"d":"0.00"}}]
[]
[22578,"7.3.1.4",null,"3) Boulder Excavation class A (Provisional)","m³",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E122 = CHAR(37), F122*G122/100,F122*G122)","v":{"v":0,"d":"0.00"}}]
[]
[22579,"7.3.1.5",null,"4) Boulder Excavation class B (Provisional)","m³",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E124 = CHAR(37), F124*G124/100,F124*G124)","v":{"v":0,"d":"0.00"}}]
[]
[22580,"7.3.1.6",null,"Hand excavation and backfill where ordered by the Engineer (Provisional Quantity)","m³",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E126 = CHAR(37), F126*G126/100,F126*G126)","v":{"v":0,"d":"0.00"}}]
[]
[22581,"7.3.1.7","8.3.2 (c)","Excavate and dispose of unsuitable material from trench bottom (Provisional)","m³",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E128 = CHAR(37), F128*G128/100,F128*G128)","v":{"v":0,"d":"0.00"}}]
[]
[22582,"7.3.1.8",null,"Hand excavation to prove existing services (Provisional)","m³",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E130 = CHAR(37), F130*G130/100,F130*G130)","v":{"v":0,"d":"0.00"}}]
[]
[22568,"7.3.2","8.3.3","EXCAVATION ANCILLARIES "]
[]
[22569,null,null,"Make up deficiency in backfill material (Provisional)"]
[]
[22570,"7.3.2.1","8.3.3.1 (a)","a) from other necessary excavations on site","m³",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E136 = CHAR(37), F136*G136/100,F136*G136)","v":{"v":0,"d":"0.00"}}]
[]
[22571,"7.3.2.2","8.3.3.1 (c)","b) by importation from commercial sources","m³",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E138 = CHAR(37), F138*G138/100,F138*G138)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":11}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H106:H149)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 7 - SECURITY GUARD HOUSE"]
[{"$nulls":7},"SECTION 7.4: BEDDING"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[22583,"7.4","SABS 1200 LB","BEDDING (PIPES)"]
[]
[22591,"7.4.1","PSLB 8.2.1","Provision of bedding from trench excavations:"]
[]
[22584,"7.4.1.1",null,"Selected granular material for 200mm bedding cradle below pipe invert","m³",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E158 = CHAR(37), F158*G158/100,F158*G158)","v":{"v":0,"d":"0.00"}}]
[]
[22585,"7.4.1.2",null,"Selected granular material for fill blanket to 300mm above pipe crown","m³",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E160 = CHAR(37), F160*G160/100,F160*G160)","v":{"v":0,"d":"0.00"}}]
[]
[22587,"7.4.1.3","PSLB 8.2.1.1","Extra Over for screening of material from the trench excavation, to achieve grading suitable to comply with the bedding and blanket material specification (Provisional Quantity) ","m³",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E162 = CHAR(37), F162*G162/100,F162*G162)","v":{"v":0,"d":"0.00"}}]
[]
[22588,"7.4.2","PSLB 8.2.2","Supply only of bedding by importation:"]
[]
[22589,null,"PSLB 8.2.2.3","From commercial sources:"]
[]
[22590,"7.4.2.1",null,"a) Selected granular material for 200mm bedding cradle below pipe invert","m³",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E168 = CHAR(37), F168*G168/100,F168*G168)","v":{"v":0,"d":"0.00"}}]
[]
[22586,"7.4.2.2",null,"b) Selected granular material for fill blanket to 300mm above pipe crown","m³",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E170 = CHAR(37), F170*G170/100,F170*G170)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":33}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H154:H203)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 7 - SECURITY GUARD HOUSE"]
[{"$nulls":7},"SECTION 7.5: CONCRETE (STRUCTURAL)"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[21677,"7.5","SANS 1200 G, PSG","CONCRETE (STRUCTURAL)"]
[]
[21678,"7.5.1","8.2","FORMWORK"]
[]
[21770,null,"8.2.1","Narrow Widths, Smooth finish from formwork on:"]
[]
[21771,null,null,"Vertical plane to"]
[]
[21772,"7.5.1.1",null,"150mm high, roof slab","m",{"v":16,"d":"16.0"},{"v":0,"d":"0.00"},{"$f":"IF(E216 = CHAR(37), F216*G216/100,F216*G216)","v":{"v":0,"d":"0.00"}}]
[]
[21958,"7.5.1.2",null,"150mm high, floor slab","m",{"v":13,"d":"13.0"},{"v":0,"d":"0.00"},{"$f":"IF(E218 = CHAR(37), F218*G218/100,F218*G218)","v":{"v":0,"d":"0.00"}}]
[]
[21975,"7.5.1.3",null,"230mm high, footings","m",{"v":27,"d":"27.0"},{"v":0,"d":"0.00"},{"$f":"IF(E220 = CHAR(37), F220*G220/100,F220*G220)","v":{"v":0,"d":"0.00"}}]
[]
[21976,"7.5.1.4",null,"75mm high, blinding layer","m",{"v":27,"d":"27.0"},{"v":0,"d":"0.00"},{"$f":"IF(E222 = CHAR(37), F222*G222/100,F222*G222)","v":{"v":0,"d":"0.00"}}]
[]
[22592,"7.5.1.5",null,"100mm high, upstand beam","m",{"v":14,"d":"14.00"},{"v":0,"d":"0.00"},{"$f":"IF(E224 = CHAR(37), F224*G224/100,F224*G224)","v":{"v":0,"d":"0.00"}}]
[]
[21679,null,null,"Smooth finish from formwork on:"]
[]
[21728,null,"8.2.2, PSG 8.2.2\r\nPSG 5.2","Horizontal plane to"]
[]
[21729,"7.5.1.6",null,"Roof slab soffit","m²",{"v":21,"d":"21.0"},{"v":0,"d":"0.00"},{"$f":"IF(E230 = CHAR(37), F230*G230/100,F230*G230)","v":{"v":0,"d":"0.00"}}]
[]
[21680,"7.5.2","8.3, PSG 8.1.2","REINFORCEMENT"]
[]
[21730,null,"8.3.1","Steel bars of various sizes"]
[]
[21681,"7.5.2.1",null,"High-tensile steel bars","t",{"v":6,"d":"6.0"},{"v":0,"d":"0.00"},{"$f":"IF(E236 = CHAR(37), F236*G236/100,F236*G236)","v":{"v":0,"d":"0.00"}}]
[]
[22593,"7.5.2.2",null,"Mild Steel Bars","t",{"v":0.6,"d":"0.60"},{"v":0,"d":"0.00"},{"$f":"IF(E238 = CHAR(37), F238*G238/100,F238*G238)","v":{"v":0,"d":"0.00"}}]
[]
[21682,"7.5.3","8.4","CONCRETE"]
[]
[21961,null,"8.4.2","Grade Concrete (15 MPa/19mm):"]
[]
[21756,"7.5.3.1",null,"Blinding layer minimum 75mm thick","m²",0.7,{"v":0,"d":"0.00"},{"$f":"IF(E244 = CHAR(37), F244*G244/100,F244*G244)","v":{"v":0,"d":"0.00"}}]
[]
[21962,null,"8.4.3, PSG 5.5","Strength Concrete:"]
[]
[21963,null,"8.4.3, PSG 5.5","Grade Concrete (25 MPa/19mm):"]
[]
[21767,"7.5.3.2",null,"85mm thick floor slab","m³",0.9,{"v":0,"d":"0.00"},{"$f":"IF(E250 = CHAR(37), F250*G250/100,F250*G250)","v":{"v":0,"d":"0.00"}}]
[]
[21748,"7.5.3.3",null,"100mm thick roof slab","m³",{"v":4,"d":"4.0"},{"v":0,"d":"0.00"},{"$f":"IF(E252 = CHAR(37), F252*G252/100,F252*G252)","v":{"v":0,"d":"0.00"}}]
[]
[21735,"7.5.3.4",null,"110mm thick footing (internal walls)","m³",{"v":1,"d":"1.0"},{"v":0,"d":"0.00"},{"$f":"IF(E254 = CHAR(37), F254*G254/100,F254*G254)","v":{"v":0,"d":"0.00"}}]
[]
[21768,"7.5.3.5",null,"700mm wide footing ","m³",{"v":3,"d":"3.0"},{"v":0,"d":"0.00"},{"$f":"IF(E256 = CHAR(37), F256*G256/100,F256*G256)","v":{"v":0,"d":"0.00"}}]
[]
[21964,"7.5.4","8.4.4","UNFORMED SURFACE FINISHES"]
[]
[21965,null,"8.4.4 (a)","Steel-floated finish to:"]
[]
[21731,"7.5.4.1",null,"Blinding","m²",{"v":9,"d":"9.0"},{"v":0,"d":"0.00"},{"$f":"IF(E262 = CHAR(37), F262*G262/100,F262*G262)","v":{"v":0,"d":"0.00"}}]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H208:H262)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 7 - SECURITY GUARD HOUSE"]
[{"$nulls":7},"SECTION 7.5: CONCRETE (STRUCTURAL)"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H263","v":{"v":0,"d":"0.00"}}]
[21864,"7.5.4.2",null,"Roof Slab","m²",{"v":21,"d":"21.0"},{"v":0,"d":"0.00"},{"$f":"IF(E268 = CHAR(37), F268*G268/100,F268*G268)","v":{"v":0,"d":"0.00"}}]
[]
[21732,"7.5.4.3",null,"Floor Slab","m²",{"v":10,"d":"10.0"},{"v":0,"d":"0.00"},{"$f":"IF(E270 = CHAR(37), F270*G270/100,F270*G270)","v":{"v":0,"d":"0.00"}}]
[]
[21733,"7.5.5",null,"WATERPROOFING"]
[]
[21865,null,null,"One layer of Derbigum SP (Special Polyester) waterproof sheeting sealed "]
[]
[21734,"7.5.5.1",null,"Top of the roof","m²",{"v":20,"d":"20.0"},{"v":0,"d":"0.00"},{"$f":"IF(E276 = CHAR(37), F276*G276/100,F276*G276)","v":{"v":0,"d":"0.00"}}]
[]
[21758,null,"8.4.4 a)","Steel-floated finish to top of:"]
[]
[21759,"7.5.5.2",null,"Roof slab ","m²",{"v":20,"d":"20.0"},{"v":0,"d":"0.00"},{"$f":"IF(E280 = CHAR(37), F280*G280/100,F280*G280)","v":{"v":0,"d":"0.00"}}]
[]
[21769,"7.5.5.3",null,"Floor slab","m²",{"v":9,"d":"9.0"},{"v":0,"d":"0.00"},{"$f":"IF(E282 = CHAR(37), F282*G282/100,F282*G282)","v":{"v":0,"d":"0.00"}}]
[]
[21843,"7.5.6","PSG 5.5.8, PSG 8.4.7","CURING AND PROTECTION"]
[]
[21844,"7.5.6.1",null,"Floor slabs","m²",{"v":9,"d":"9.0"},{"v":0,"d":"0.00"},{"$f":"IF(E286 = CHAR(37), F286*G286/100,F286*G286)","v":{"v":0,"d":"0.00"}}]
[]
[21845,"7.5.6.2",null,"Roof slab","m²",{"v":20,"d":"20.0"},{"v":0,"d":"0.00"},{"$f":"IF(E288 = CHAR(37), F288*G288/100,F288*G288)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":35}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H267:H323)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 7 - SECURITY GUARD HOUSE"]
[{"$nulls":7},"SECTION 7.6: METALWORK"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[22644,"7.6","SANS 1200 H, PSHA, PACP","METALWORK"]
[]
[22645,"7.6.1",null,"SUPPLEMENTARY PREAMBLES"]
[]
[22646,null,null,"The following to be finished with 25 microns powder coated, manufactured and installed in accordance with good building practice and in terms of the latest code of practice with revisions as recommended by SANS and AAAMSA"]
[]
[22647,null,null,"Items shall be manufactured by an approved specialist who shall provide a sample upon request, for the Engineers approval"]
[]
[22648,null,null,"Tenderers are advised to refer to the Architect's window and door schedules attached to these Bills of Quantities for details on drawing 60398/25"]
[]
[22649,null,null,"Tenderers are to note that should there be any doubt or obscurity as to the meaning and intent of any descriptions, the Contractor must have the same rectified and allow for same accordingly in his tender. The Contractor is to include in his rates for all that he considers necessary for the proper construction of the windows and doors. No claims whatsoever will be afterwards admitted due to the Contractor having failed to comply with these conditions"]
[]
[22650,null,null,"Rates shall include for the following:"]
[]
[22651,null,null,"1. All opening and fixed lights, coupling mullions and transoms, support steelwork, fittings, ironmongery, etc., as required and specified."]
[]
[22652,null,null,"2. Complete glazing as described, with and including matching aluminium glazing beads and gaskets and glazed in accordance with the manufacturer's written instructions"]
[]
[]
[]
[]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H328:H349)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 7 - SECURITY GUARD HOUSE"]
[{"$nulls":7},"SECTION 7.6: METALWORK"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H350","v":{"v":0,"d":"0.00"}}]
[22653,null,null,"3. Building in and fixing into preformed openings. Window opening sizes to be verified on site before windows can be manufactured"]
[]
[22654,null,null,"4. Suitably protecting all exposed aluminium and glass surfaces with an approved protection tape and plastic sheeting. Such protection is to be removed at completion of the contract and the exposed surfaces cleaned down and left perfect. Under no circumstances will any damage whatsoever to the finished product be acceptable"]
[]
[22655,null,null,"5. Silicone pointing with a silicone sealant recommended by AAAMSA on all door / window and structure junctions"]
[]
[22656,"7.6.2",null,"NATURAL ANODISED ALUMINIUM WINDOWS, DOORS, ETC."]
[]
[22666,null,null,"Note: Tenderers are to refer to the Architects door schedules when pricing the items hereunder"]
[]
[22657,null,null,"Hardwood Meranti door frames plugged to brickwork "]
[]
[22658,"7.6.2.1",null,"WD01","No.",{"v":2,"d":"2.0"},{"v":0,"d":"0.00"},{"$f":"IF(E367 = CHAR(37), F367*G367/100,F367*G367)","v":{"v":0,"d":"0.00"}}]
[]
[22659,null,null,"Note: Tenderers are to refer to the attached Architects window schedules when pricing the items hereunder"]
[]
[22660,null,null,"Wispeco/similar standard aluminium window frame plugged to brickwork or concrete, complete with burglar bars"]
[]
[22661,"7.6.2.2",null,"AW01","No.",{"v":2,"d":"2.0"},{"v":0,"d":"0.00"},{"$f":"IF(E373 = CHAR(37), F373*G373/100,F373*G373)","v":{"v":0,"d":"0.00"}}]
[]
[22665,"7.6.2.3",null,"AW02","No.",{"v":1,"d":"1.0"},{"v":0,"d":"0.00"},{"$f":"IF(E375 = CHAR(37), F375*G375/100,F375*G375)","v":{"v":0,"d":"0.00"}}]
[]
[22677,"7.6.2.4",null,"AW03","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E377 = CHAR(37), F377*G377/100,F377*G377)","v":{"v":0,"d":"0.00"}}]
[]
[22673,null,null,"Tinted glass"]
[]
[22674,"7.6.2.5",null,"Allow for all external glass windows and doors to be tinted with 20%, 2-ply, non-reflective film","Sum",{"v":1,"d":"1.0"},{"v":0,"d":"0.00"},{"$f":"IF(E381 = CHAR(37), F381*G381/100,F381*G381)","v":{"v":0,"d":"0.00"}}]
[]
[22675,"7.6.2.6",null,"Allow for glass awareness decals on all doors","Sum",{"v":1,"d":"1.0"},{"v":0,"d":"0.00"},{"$f":"IF(E383 = CHAR(37), F383*G383/100,F383*G383)","v":{"v":0,"d":"0.00"}}]
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H354:H383)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 7 - SECURITY GUARD HOUSE"]
[{"$nulls":7},"SECTION 7.7: MASONRY"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[21683,"7.7","SANS 1200 H, PSAHA, PACP","MASONRY"]
[]
[21977,null,null,"SUPPLEMENTARY PREAMBLES:"]
[]
[21978,null,null,"Sizes in descriptions"]
[]
[21979,null,null,"Where sizes in descriptions are given in brick units, 'one brick' shall represent the length and 'half brick' the width of a brick."]
[]
[21980,null,null,"Hollow walls, etc"]
[]
[21981,null,null,"Descriptions of hollow walls shall be deemed to include leaving every fifth perpend of the bottom course of the external skin open as a weep hole."]
[]
[21982,null,null,"Walls in two skins described as 'bagged and sealed' shall be deemed to include having the outer face of the inner skin bagged with 1:6 cement and sand mixture"]
[]
[21983,null,null,"Face bricks"]
[]
[21984,null,null,"Bricks shall be ordered timeously to obtain uniformity in size and colour"]
[]
[21985,null,null,"Pointing"]
[]
[21986,null,null,"Descriptions of recessed pointing to fair face brickwork and face brickwork shall be deemed to include square recessed, hollow recessed, weathered pointing, etc."]
[]
[21987,"7.7.1","PABR","BRICKWORK IN SUPERSTRUCTURE"]
[]
[21988,null,null,"In mortar class according to PABR 2.6:"]
[]
[21992,null,null,"Proposed Guard House"]
[]
[21993,null,null,"New external one brick walls in Roan Satin FBX facebrick skin externally with common NFP brick skin internally to be plastered and painted (measured elsewhere)"]
[]
[21994,"7.7.1.1",null,"External facebrick skin ","m²",{"v":35,"d":"35.0"},{"v":0,"d":"0.00"},{"$f":"IF(E418 = CHAR(37), F418*G418/100,F418*G418)","v":{"v":0,"d":"0.00"}}]
[]
[21995,"7.7.1.2",null,"Internal common brick skin ","m²",{"v":35,"d":"35.0"},{"v":0,"d":"0.00"},{"$f":"IF(E420 = CHAR(37), F420*G420/100,F420*G420)","v":{"v":0,"d":"0.00"}}]
[]
[]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H388:H423)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 7 - SECURITY GUARD HOUSE"]
[{"$nulls":7},"SECTION 7.7: MASONRY"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H424","v":{"v":0,"d":"0.00"}}]
[21996,null,null,"New internal walls in common NFP brickwork to be plastered and painted (measured elsewhere)"]
[]
[21997,"7.7.1.3",null,"Single skin wall ","m²",{"v":5,"d":"5.0"},{"v":0,"d":"0.00"},{"$f":"IF(E431 = CHAR(37), F431*G431/100,F431*G431)","v":{"v":0,"d":"0.00"}}]
[]
[21999,"7.7.2","PABR","BRICKWORK SUNDRIES"]
[]
[22000,null,null,"Brick on edge lintels"]
[]
[22001,"7.7.2.1",null,"110 x 150mm lintels in lengths not exceeding 3m","m",{"v":6,"d":"6.0"},{"v":0,"d":"0.00"},{"$f":"IF(E437 = CHAR(37), F437*G437/100,F437*G437)","v":{"v":0,"d":"0.00"}}]
[]
[22002,null,null,"Brick on edge sills"]
[]
[22003,"7.7.2.2",null,"110 x 150mm sills in lengths not exceeding 3m","m",{"v":5,"d":"5.0"},{"v":0,"d":"0.00"},{"$f":"IF(E441 = CHAR(37), F441*G441/100,F441*G441)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":41}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H428:H482)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 7 - SECURITY GUARD HOUSE"]
[{"$nulls":7},"SECTION 7.8: PLASTERING"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[22594,"7.8","PABR 5.3.1\r\nPABR 2.1","PLASTERING"]
[]
[22595,"7.8.1",null,"PRICES"]
[]
[22596,null,null,"The prices of mouldings, weathering, skirting, labours, etc. shall include for forming mitres, stops, etc. unless otherwise described"]
[]
[22597,null,null,"The prices of all rendering shall include for working around pipes, balusters, etc"]
[]
[22598,null,null,"Rates for plaster are to include for all filling to and working around electrical conduits, etc., prior to plastering"]
[]
[22602,"7.8.2",null,"INTERNAL PLASTER"]
[]
[22603,null,null,"One coat cement plaster on brickwork:"]
[]
[22604,"7.8.2.1",null,"Walls","m²",{"v":32,"d":"32.0"},{"v":0,"d":"0.00"},{"$f":"IF(E501 = CHAR(37), F501*G501/100,F501*G501)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":34}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H487:H535)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 7 - SECURITY GUARD HOUSE"]
[{"$nulls":7},"SECTION 7.9: PAINTING"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[22614,"7.9",null,"PAINTING"]
[]
[22615,"7.9.1",null,"PREPARATORY WORK TO EXISTING WORK"]
[]
[22616,null,null,"Previously painted plastered surfaces:"]
[]
[22617,null,null,"Surfaces shall be thoroughly washed down and allowed to dry completely before any paint is applied. Blistered or peeling paint shall be completely removed and cracks shall be opened, filled with a suitable filler and finished smooth"]
[]
[22618,null,null,"Previously painted metal surfaces:"]
[]
[22605,null,null,"Surfaces shall be thoroughly rubbed and cleaned down. Blistered or peeling paint shall be completely removed down to bare metal"]
[]
[22606,null,null,"Previously painted wood surfaces:"]
[]
[22607,null,null,"Surfaces shall be thoroughly cleaned down. Blistered or peeling paint shall be completely removed and cracks and crevices shall be primed, filled with suitable filler and finished smooth"]
[]
[22611,"7.9.2",null,"PAINTWORK, ETC. TO NEW WORK ON INTERNAL FLOATED PLASTERED SURFACES"]
[]
[22612,null,null,"One coat plaster primer, one undercoat and two finishing coats non drip enamel for interior application"]
[]
[22613,"7.9.2.1",null,"On internal Walls","m²",{"v":32,"d":"32.0"},{"v":0,"d":"0.00"},{"$f":"IF(E560 = CHAR(37), F560*G560/100,F560*G560)","v":{"v":0,"d":"0.00"}}]
[]
[22619,"7.9.3",null,"PAINTWORK, ETC. TO NEW WORK ON INTERNAL CEILING SURFACES"]
[]
[22620,null,null,"One coat plaster primer, one undercoat and two finishing coats non drip enamel for interior application"]
[]
[22621,"7.9.3.1",null,"On ceiling of existing and new buildings","m²",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E566 = CHAR(37), F566*G566/100,F566*G566)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":7}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H540:H573)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 7 - SECURITY GUARD HOUSE"]
[{"$nulls":7},"SECTION 7.10: PROVISIONAL SUMS"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[23088,"7.10",null,"PROVISIONAL SUMS"]
[]
[23089,null,null,"Signage"]
[]
[23090,"7.10.1",null,"Supply and install signage ","Prov Sum",{"v":1,"d":"1.0"},{"v":5000,"d":"5,000.00"},{"v":5000,"d":"5,000.00"}]
[]
[23091,"7.10.2",null,"Overheads, charges and profit on above item 7.10.1","%",{"$f":"H582","v":{"v":5000,"d":"5,000.0"}},{"v":0,"d":"0.00"},{"$f":"IF(E584 = CHAR(37), F584*G584/100,F584*G584)","v":{"v":0,"d":"0.00"}}]
[]
[23092,null,null,"Guard House wash hand basins and sinks"]
[]
[23093,"7.10.3",null,"Supply and install wash hand basins and sinks","Prov Sum",{"v":1,"d":"1.0"},{"v":5000,"d":"5,000.00"},{"v":5000,"d":"5,000.00"}]
[]
[23094,"7.10.4",null,"Overheads, charges and profit on above item 7.10.3","%",{"$f":"H588","v":{"v":5000,"d":"5,000.0"}},{"v":0,"d":"0.00"},{"$f":"IF(E590 = CHAR(37), F590*G590/100,F590*G590)","v":{"v":0,"d":"0.00"}}]
[]
[23095,null,null,"Guard House ablution facilities"]
[]
[23096,"7.10.5",null,"Supply and install toilets","Prov Sum",{"v":1,"d":"1.0"},{"v":7500,"d":"7,500.00"},{"v":7500,"d":"7,500.00"}]
[]
[23097,"7.10.6",null,"Overheads, charges and profit on above item 7.10.5","%",{"$f":"H594","v":{"v":7500,"d":"7,500.0"}},{"v":0,"d":"0.00"},{"$f":"IF(E596 = CHAR(37), F596*G596/100,F596*G596)","v":{"v":0,"d":"0.00"}}]
[]
[23098,null,null,"Guard House water supply"]
[]
[23099,"7.10.7",null,"Supply and install water supply","Prov Sum",{"v":1,"d":"1.0"},{"v":10000,"d":"10,000.00"},{"v":10000,"d":"10,000.00"}]
[]
[23100,"7.10.8",null,"Overheads, charges and profit on above item 7.10.7","%",{"$f":"H600","v":{"v":10000,"d":"10,000.0"}},{"v":0,"d":"0.00"},{"$f":"IF(E602 = CHAR(37), F602*G602/100,F602*G602)","v":{"v":0,"d":"0.00"}}]
[]
[23107,null,"C5.2.6","Sewer Installation"]
[]
[23108,"7.10.9",null,"Supply and install sewer connection and associated works","Prov Sum",{"v":1,"d":"1.0"},{"v":10000,"d":"10,000.00"},{"v":10000,"d":"10,000.00"}]
[]
[23109,"7.10.10",null,"Overheads, charges and profit on above item 7.10.9","%",{"$f":"H606","v":{"v":10000,"d":"10,000.0"}},{"v":0,"d":"0.00"},{"$f":"IF(E608 = CHAR(37), F608*G608/100,F608*G608)","v":{"v":0,"d":"0.00"}}]
[]
[23104,null,null,"Furniture for Guard House"]
[]
[23105,"7.10.11",null,"Supply and install furniture for offices, labs, boardrooms, workshop, control room, and kitchen","Prov Sum",{"v":1,"d":"1.0"},{"v":15000,"d":"15,000.00"},{"v":15000,"d":"15,000.00"}]
[]
[23106,"7.10.12",null,"Overheads, charges and profit on above item 7.10.11","%",{"$f":"H612","v":{"v":15000,"d":"15,000.0"}},{"v":0,"d":"0.00"},{"$f":"IF(E614 = CHAR(37), F614*G614/100,F614*G614)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":9}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H578:H623)","v":{"v":52500,"d":"52,500.00"}}]
[null,"SCHEDULE 7 - SECURITY GUARD HOUSE"]
[{"$nulls":7},"SECTION 7.11: GENERAL"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[21859,"7.11",null,"GENERAL ITEMS"]
[]
[21917,"7.11.1",null,"SIGNAGE"]
[]
[21871,"7.11.1.1",null,"Supply and install signage as directed by the Engineer","Prov Sum",{"v":1,"d":"1.0"},{"v":15000,"d":"15,000.00"},{"v":15000,"d":"15,000.00"}]
[]
[21872,"7.11.1.2",null,"Overheads, charges and profit on above item 7.11.1.1","%",{"$f":"H632","v":{"v":15000,"d":"15,000.0"}},{"v":0,"d":"0.00"},{"$f":"IF(E634 = CHAR(37), F634*G634/100,F634*G634)","v":{"v":0,"d":"0.00"}}]
[]
[21918,"7.11.2",null,"GENERAL"]
[]
[21860,null,null,"Any other item the tenderer considers has been omitted and which requires pricing as separate items."]
[]
[21861,"7.11.2.1",null,"i)","Sum",{"v":1,"d":"1.0"},{"v":0,"d":"0.00"},{"$f":"IF(E640 = CHAR(37), F640*G640/100,F640*G640)","v":{"v":0,"d":"0.00"}}]
[]
[21862,"7.11.2.2",null,"ii)","Sum",{"v":1,"d":"1.0"},{"v":0,"d":"0.00"},{"$f":"IF(E642 = CHAR(37), F642*G642/100,F642*G642)","v":{"v":0,"d":"0.00"}}]
[]
[21863,"7.11.2.3",null,"iii)","Sum",{"v":1,"d":"1.0"},{"v":0,"d":"0.00"},{"$f":"IF(E644 = CHAR(37), F644*G644/100,F644*G644)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":38}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H628:H682)","v":{"v":15000,"d":"15,000.00"}}]
[null,"SCHEDULE 7 - SECURITY GUARD HOUSE"]
[{"$nulls":3},"SUMMARY OF SECTIONS"]
[null," ","SECTION","DESCRIPTION",{"$nulls":3},"AMOUNT\n(RAND)"]
[null,null,"7.1","SECTION 7.1: SITE CLEARANCE",{"$nulls":3},{"$f":"H52","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"7.2","SECTION 7.2: EARTHWORKS",{"$nulls":3},{"$f":"H102","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"7.3","SECTION 7.3: EARTHWORKS (PIPE TRENCHES)",{"$nulls":3},{"$f":"H150","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"7.4","SECTION 7.4: BEDDING",{"$nulls":3},{"$f":"H204","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"7.5","SECTION 7.5: CONCRETE (STRUCTURAL)",{"$nulls":3},{"$f":"H324","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"7.6","SECTION 7.6: METALWORK",{"$nulls":3},{"$f":"H384","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"7.7","SECTION 7.7: MASONRY",{"$nulls":3},{"$f":"H483","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"7.8","SECTION 7.8: PLASTERING",{"$nulls":3},{"$f":"H536","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"7.9","SECTION 7.9: PAINTING",{"$nulls":3},{"$f":"H574","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"7.10","SECTION 7.10: PROVISIONAL SUMS",{"$nulls":3},{"$f":"H624","v":{"v":52500,"d":"52,500.00"}}]
[]
[null,null,"7.11","SECTION 7.11: GENERAL",{"$nulls":3},{"$f":"H683","v":{"v":15000,"d":"15,000.00"}}]
{"$rows_empty":37}
[null,null," Total Carried Forward To Summary Of Schedules"," Total Carried Forward To Summary Of Schedules",{"$nulls":3},{"$f":"SUM(H687:H744)","v":{"v":67500,"d":"67,500.00"}}]

{"sheet":"Schedule 8","index":7,"n_rows":1164,"n_cols":8,"rows_kept":1164}
["Rate=G","SCHEDULE 8 - BACKWASH, SLUDGE AND BACKWASH RECOVERY SYSTEMS & "]
[null,"CHAMBERS"]
[{"$nulls":7},"SECTION 8.1: SITE CLEARANCE"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[22021,"8.1","SANS 1200 C, PSC & PSDB","SITE CLEARANCE"]
[]
[22218,null,null,"All drawing references are prefixed with 60398/02 - 60398/09"]
[]
[22231,"8.1.1",null,"DN250 In-Situ Chamber"]
[]
[22110,"8.1.1.1","PSC8.2.11","Saw cutting of existing asphalt surface","m",{"v":27,"d":"27.0"},{"v":0,"d":"0.00"},{"$f":"IF(E11 = CHAR(37), F11*G11/100,F11*G11)","v":{"v":0,"d":"0.00"}}]
[]
[22114,"8.1.1.2","PSC8.2.13","Remove existing road asphalt surfacing and spoil at approved spoil disposal site up to 60mm thickness","m²",{"v":3,"d":"3.0"},{"v":0,"d":"0.00"},{"$f":"IF(E13 = CHAR(37), F13*G13/100,F13*G13)","v":{"v":0,"d":"0.00"}}]
[]
[22236,"8.1.2",null,"DN80 Residue Sludge Disposal "]
[]
[22023,"8.1.2.1","8.2.1, PSC 8.2.1","Clear and Grub Site","m²",{"v":19,"d":"19.0"},{"v":0,"d":"0.00"},{"$f":"IF(E17 = CHAR(37), F17*G17/100,F17*G17)","v":{"v":0,"d":"0.00"}}]
[]
[22235,"8.1.3",null,"DN100 IV Precast Concrete Chamber"]
[]
[22233,"8.1.3.1","8.2.1, PSC 8.2.1","Clear and Grub Site","m²",{"v":23,"d":"23.0"},{"v":0,"d":"0.00"},{"$f":"IF(E21 = CHAR(37), F21*G21/100,F21*G21)","v":{"v":0,"d":"0.00"}}]
[]
[22116,"8.1.4","8.2.10, PSC 8.2.10","Remove topsoil to depth of 150mm and stockpile for all chamber","m³",{"v":10,"d":"10.0"},{"v":0,"d":"0.00"},{"$f":"IF(E23 = CHAR(37), F23*G23/100,F23*G23)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":33}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H5:H56)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 8 - BACKWASH, SLUDGE AND BACKWASH RECOVERY SYSTEMS & "]
[null,"CHAMBERS"]
[{"$nulls":7},"SECTION 8.2: EARTHWORKS"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[22024,"8.2","SANS 1200 D, PSD","EARTHWORKS"]
[]
[22069,"8.2.1","8.3.3, PSD 8.3.3(a), PSD 2.3","RESTRICTED EXCAVATION"]
[]
[22025,null,"8.3.3 a), PSD 8.3.5.2","Restricted excavation in all materials and stockpile suitable material and use for embankment or backfill, and dispose of unsuitable material to an approved spoil site to be determined by the contractor"]
[]
[22026,"8.2.1.1",null,"DN250 In-Situ Chamber","m³",{"v":94,"d":"94.0"},{"v":0,"d":"0.00"},{"$f":"IF(E68 = CHAR(37), F68*G68/100,F68*G68)","v":{"v":0,"d":"0.00"}}]
[]
[22027,"8.2.1.2",null,"DN80 Residue Sludge Disposal ","m³",{"v":22,"d":"22.0"},{"v":0,"d":"0.00"},{"$f":"IF(E70 = CHAR(37), F70*G70/100,F70*G70)","v":{"v":0,"d":"0.00"}}]
[]
[22219,"8.2.1.3",null,"DN100 IV Precast Concrete Chamber","m³",{"v":28,"d":"28.0"},{"v":0,"d":"0.00"},{"$f":"IF(E72 = CHAR(37), F72*G72/100,F72*G72)","v":{"v":0,"d":"0.00"}}]
[]
[22028,null,"8.3.3 b), PSD 3.1","Extra-over items 8.2.1.1 to 8.2.1.3 for:"]
[]
[22029,"8.2.1.4","8.3.3 b) 1)","Intermediate material","m³",{"v":70,"d":"70.0"},{"v":0,"d":"0.00"},{"$f":"IF(E76 = CHAR(37), F76*G76/100,F76*G76)","v":{"v":0,"d":"0.00"}}]
[]
[22030,"8.2.1.5","8.3.3 b) 2)","Hard rock material","m³",{"v":10,"d":"10.0"},{"v":0,"d":"0.00"},{"$f":"IF(E78 = CHAR(37), F78*G78/100,F78*G78)","v":{"v":0,"d":"0.00"}}]
[]
[22031,"8.2.1.6","8.3.3 b) 3)","Boulder material, Class A (Provisional)","m³",{"v":5,"d":"5.0"},{"v":0,"d":"0.00"},{"$f":"IF(E80 = CHAR(37), F80*G80/100,F80*G80)","v":{"v":0,"d":"0.00"}}]
[]
[22032,"8.2.1.7","8.3.3 b) 4)","Boulder material, Class B (Provisional)","m³",{"v":5,"d":"5.0"},{"v":0,"d":"0.00"},{"$f":"IF(E82 = CHAR(37), F82*G82/100,F82*G82)","v":{"v":0,"d":"0.00"}}]
[]
[22117,"8.2.2","8.3.3 a)","FOUNDATION PREPARATION"]
[]
[22070,"8.2.2.1",null,"Rip & re-compact in-situ material to 98% MOD AASHTO in 150mm layers","m³",{"v":10,"d":"10.0"},{"v":0,"d":"0.00"},{"$f":"IF(E86 = CHAR(37), F86*G86/100,F86*G86)","v":{"v":0,"d":"0.00"}}]
[]
[22033,"8.2.3",null,"BACKFILL"]
[]
[22118,null,"PSD 8.3.4.1","Selected backfill or fill material obtained from stockpile"]
[]
[22119,"8.2.3.1",null,"Fill embankment around chambers compacted to 95% MOD AASHTO in 150mm layers including testing","m³",{"v":75,"d":"75.0"},{"v":0,"d":"0.00"},{"$f":"IF(E92 = CHAR(37), F92*G92/100,F92*G92)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":15}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H62:H107)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 8 - BACKWASH, SLUDGE AND BACKWASH RECOVERY SYSTEMS & "]
[null,"CHAMBERS"]
[{"$nulls":7},"SECTION 8.3: EARTHWORKS (PIPE TRENCHES)"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[22540,"8.3","SABS1200 DB","EARTHWORKS (PIPE TRENCHES)"]
[]
[22541,"8.3.1","PSDB 5.2 \r\n8.3.2","EXCAVATION"]
[]
[22546,null,"8.3.2 (a) PSDB 8.3.2 (a)","Excavate in all materials for pipe trenches, backfill, compact to specification and dispose of surplus/unsuitable material, for pipes:"]
[]
[22547,null,null,"Up to DN400 pipeline for a total trench depth"]
[]
[22548,"8.3.1.1",null,"Up to 3.0m","m³",{"v":120,"d":"120.00"},{"v":0,"d":"0.00"},{"$f":"IF(E121 = CHAR(37), F121*G121/100,F121*G121)","v":{"v":0,"d":"0.00"}}]
[]
[22549,null,"8.3.2 (b) PSDB 8.3.2 (b)","Extra-over Item 8.3.1.1 for excavation in (All provisional):"]
[]
[22550,"8.3.1.2",null,"1) Intermediate excavation","m³",{"v":60,"d":"60.00"},{"v":0,"d":"0.00"},{"$f":"IF(E125 = CHAR(37), F125*G125/100,F125*G125)","v":{"v":0,"d":"0.00"}}]
[]
[22551,"8.3.1.3",null,"2) Hard rock excavation","m³",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E127 = CHAR(37), F127*G127/100,F127*G127)","v":{"v":0,"d":"0.00"}}]
[]
[22552,"8.3.1.4",null,"3) Boulder Excavation class A (Provisional)","m³",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E129 = CHAR(37), F129*G129/100,F129*G129)","v":{"v":0,"d":"0.00"}}]
[]
[22553,"8.3.1.5",null,"4) Boulder Excavation class B (Provisional)","m³",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E131 = CHAR(37), F131*G131/100,F131*G131)","v":{"v":0,"d":"0.00"}}]
[]
[22554,"8.3.1.6",null,"Hand excavation and backfill where ordered by the Engineer (Provisional Quantity)","m³",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E133 = CHAR(37), F133*G133/100,F133*G133)","v":{"v":0,"d":"0.00"}}]
[]
[22555,"8.3.1.7","8.3.2 (c)","Excavate and dispose of unsuitable material from trench bottom (Provisional)","m³",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E135 = CHAR(37), F135*G135/100,F135*G135)","v":{"v":0,"d":"0.00"}}]
[]
[22556,"8.3.1.8",null,"Hand excavation to prove existing services (Provisional)","m³",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E137 = CHAR(37), F137*G137/100,F137*G137)","v":{"v":0,"d":"0.00"}}]
[]
[22542,"8.3.2","8.3.3","EXCAVATION ANCILLARIES "]
[]
[22543,null,null,"Make up deficiency in backfill material (Provisional)"]
[]
[22544,"8.3.2.1","8.3.3.1 (a)","a) from other necessary excavations on site","m³",{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"$f":"IF(E143 = CHAR(37), F143*G143/100,F143*G143)","v":{"v":0,"d":"0.00"}}]
[]
[22545,"8.3.2.2","8.3.3.1 (c)","b) by importation from commercial sources","m³",{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"$f":"IF(E145 = CHAR(37), F145*G145/100,F145*G145)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":11}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H113:H156)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 8 - BACKWASH, SLUDGE AND BACKWASH RECOVERY SYSTEMS & "]
[null,"CHAMBERS"]
[{"$nulls":7},"SECTION 8.4: CONCRETE (STRUCTURAL)"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[23132,"8.4","SABS 1200 G","CONCRETE (STRUCTURAL)"]
[]
[23133,"8.4.1","8.2","FORMWORK"]
[]
[23141,null,"8.2.2\r\nPSG8.2.2","Smooth Vertical Plane to:"]
[]
[23162,"8.4.1.1",null,"Chamber walls","m²",{"v":65,"d":"65.00"},{"v":0,"d":"0.00"},{"$f":"IF(E168 = CHAR(37), F168*G168/100,F168*G168)","v":{"v":0,"d":"0.00"}}]
[]
[23189,null,"8.2.2\r\nPSG8.2.2","Smooth Horizontal Plane to:"]
[]
[23190,"8.4.1.2",null,"Chamber roof","m²",{"v":11,"d":"11.00"},{"v":0,"d":"0.00"},{"$f":"IF(E172 = CHAR(37), F172*G172/100,F172*G172)","v":{"v":0,"d":"0.00"}}]
[]
[23122,null,"8.2.5","Narrow Widths, smooth vertical plane, for:"]
[]
[23163,"8.4.1.3",null,"75mm high, vertical face to chamber wall kicker","m",{"v":15,"d":"15.00"},{"v":0,"d":"0.00"},{"$f":"IF(E176 = CHAR(37), F176*G176/100,F176*G176)","v":{"v":0,"d":"0.00"}}]
[]
[23164,"8.4.1.4",null,"300mm high, vertical face for chamber floor slab","m",{"v":15,"d":"15.00"},{"v":0,"d":"0.00"},{"$f":"IF(E178 = CHAR(37), F178*G178/100,F178*G178)","v":{"v":0,"d":"0.00"}}]
[]
[23165,"8.4.1.5",null,"200mm high, vertical side for chamber access lids","m",{"v":15,"d":"15.00"},{"v":0,"d":"0.00"},{"$f":"IF(E180 = CHAR(37), F180*G180/100,F180*G180)","v":{"v":0,"d":"0.00"}}]
[]
[23166,"8.4.1.6",null,"200mm high, vertical face for chamber upstand beams","m",{"v":15,"d":"15.00"},{"v":0,"d":"0.00"},{"$f":"IF(E182 = CHAR(37), F182*G182/100,F182*G182)","v":{"v":0,"d":"0.00"}}]
[]
[23175,"8.4.1.7",null,"200mm high, vertical face to chamber roof openings","m",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E184 = CHAR(37), F184*G184/100,F184*G184)","v":{"v":0,"d":"0.00"}}]
[]
[24199,"8.4.1.8",null,"200m high, vertical face to pump plinth","m",{"v":30,"d":"30.00"},{"v":0,"d":"0.00"},{"$f":"IF(E186 = CHAR(37), F186*G186/100,F186*G186)","v":{"v":0,"d":"0.00"}}]
[]
[23176,null,"8.2.5","Narrow Widths, smooth horizontal plane, for:"]
[]
[23177,"8.4.1.9",null,"100mm wide, horizontal face to chamber roof openings","m",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E190 = CHAR(37), F190*G190/100,F190*G190)","v":{"v":0,"d":"0.00"}}]
[]
[23142,"8.4.2",null,"FORMWORK SUNDRIES"]
[]
[23143,null,"8.2.6\r\nPSG 8.2.6","Box out holes or form voids in:"]
[]
[23144,null,"8.2.6 (a)","Thickness up to and including for small, circular diameters up to and including 300mm."]
[]
[23145,"8.4.2.1","8.2.6 (a)","0m - 0,5m thick","No.",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E198 = CHAR(37), F198*G198/100,F198*G198)","v":{"v":0,"d":"0.00"}}]
[]
[23110,null,"8.2.6 (c)","Thickness up to and including for large, circular diameters from 300mm to 800mm."]
[]
[23111,"8.4.2.2","8.2.6 (c)","0m - 0,5m thick","No.",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"$f":"IF(E202 = CHAR(37), F202*G202/100,F202*G202)","v":{"v":0,"d":"0.00"}}]
[]
[23112,null,"8.2.6 (d)","Thickness up to and including for large, other shapes, area 0,1 - 0,5 m²"]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H162:H205)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 8 - BACKWASH, SLUDGE AND BACKWASH RECOVERY SYSTEMS & "]
[null,"CHAMBERS"]
[{"$nulls":7},"SECTION 8.4: CONCRETE (STRUCTURAL)"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H206","v":{"v":0,"d":"0.00"}}]
[23113,"8.4.2.3","8.2.6 (d)","0m - 0,5m thick","No.",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"$f":"IF(E212 = CHAR(37), F212*G212/100,F212*G212)","v":{"v":0,"d":"0.00"}}]
[]
[23114,"8.4.3","8.3\r\nPSG 8.1.2","REINFORCEMENT"]
[]
[23115,"8.4.3.1","8.3.1","Mild steel bars","t",{"v":0.3,"d":"0.30"},{"v":0,"d":"0.00"},{"$f":"IF(E216 = CHAR(37), F216*G216/100,F216*G216)","v":{"v":0,"d":"0.00"}}]
[]
[23116,"8.4.3.2","8.3.1","High-tensile steel bars","t",{"v":3,"d":"3.00"},{"v":0,"d":"0.00"},{"$f":"IF(E218 = CHAR(37), F218*G218/100,F218*G218)","v":{"v":0,"d":"0.00"}}]
[]
[23150,"8.4.3.3","8.3.2","High-tensile weld mesh","m²",{"v":15,"d":"15.00"},{"v":0,"d":"0.00"},{"$f":"IF(E220 = CHAR(37), F220*G220/100,F220*G220)","v":{"v":0,"d":"0.00"}}]
[]
[23120,"8.4.4","8.4","CONCRETE"]
[]
[23117,null,"8.4.2\r\nPSG 5.5\r\n","Grade Concrete (15 Mpa/19mm):"]
[]
[23118,"8.4.4.1",null,"Blinding layer minimum 75mm thick for below chambers","m³",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E226 = CHAR(37), F226*G226/100,F226*G226)","v":{"v":0,"d":"0.00"}}]
[]
[23119,null,"8.4.3\r\nPSG 5.5","Strength Concrete - Grade Concrete (25 Mpa/19mm):"]
[]
[23156,"8.4.4.2",null,"Chamber floors","m³",{"v":6,"d":"6.00"},{"v":0,"d":"0.00"},{"$f":"IF(E230 = CHAR(37), F230*G230/100,F230*G230)","v":{"v":0,"d":"0.00"}}]
[]
[23157,"8.4.4.3",null,"Chamber walls","m³",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E232 = CHAR(37), F232*G232/100,F232*G232)","v":{"v":0,"d":"0.00"}}]
[]
[23158,"8.4.4.4",null,"Chamber Roof","m³",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E234 = CHAR(37), F234*G234/100,F234*G234)","v":{"v":0,"d":"0.00"}}]
[]
[24200,"8.4.4.5",null,"Pump Plinths","m³",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E236 = CHAR(37), F236*G236/100,F236*G236)","v":{"v":0,"d":"0.00"}}]
[]
[23146,null,"8.4.3\r\nPSG 5.5\r\nPSG 8.4.7","Strength Concrete - Grade Concrete (25 Mpa/19mm) complete, for:"]
[]
[23147,"8.4.4.6",null,"Removable chamber lids for chambers","m³",{"v":6,"d":"6.00"},{"v":0,"d":"0.00"},{"$f":"IF(E240 = CHAR(37), F240*G240/100,F240*G240)","v":{"v":0,"d":"0.00"}}]
[]
[23134,"8.4.5","8.4.4\r\nPSG 5.2.1","UNFORMED SURFACE FINISHES"]
[]
[23135,null,"8.4.4 (a)","Wood-floated finish to:"]
[]
[23126,"8.4.5.1",null,"Blinding","m²",{"v":20,"d":"20.00"},{"v":0,"d":"0.00"},{"$f":"IF(E246 = CHAR(37), F246*G246/100,F246*G246)","v":{"v":0,"d":"0.00"}}]
[]
[23136,null,"8.4.4 (b)","Steel-floated finish to:"]
[]
[23131,"8.4.5.2",null,"Top of chamber walls","m²",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E250 = CHAR(37), F250*G250/100,F250*G250)","v":{"v":0,"d":"0.00"}}]
[]
[23148,"8.4.5.3",null,"Top of Chamber Roof Slab","m²",{"v":8,"d":"8.00"},{"v":0,"d":"0.00"},{"$f":"IF(E252 = CHAR(37), F252*G252/100,F252*G252)","v":{"v":0,"d":"0.00"}}]
[]
[23191,"8.4.5.4",null,"Top of Chamber Floor Slab","m²",{"v":12,"d":"12.00"},{"v":0,"d":"0.00"},{"$f":"IF(E254 = CHAR(37), F254*G254/100,F254*G254)","v":{"v":0,"d":"0.00"}}]
[]
[24201,"8.4.5.5",null,"Top of pump plinth","m²",{"v":30,"d":"30.00"},{"v":0,"d":"0.00"},{"$f":"IF(E256 = CHAR(37), F256*G256/100,F256*G256)","v":{"v":0,"d":"0.00"}}]
[]
[23137,"8.4.6","8.5\r\n5.5.7\r\nPSG 5.5.7\r\n","JOINTS"]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H211:H258)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 8 - BACKWASH, SLUDGE AND BACKWASH RECOVERY SYSTEMS & "]
[null,"CHAMBERS"]
[{"$nulls":7},"SECTION 8.4: CONCRETE (STRUCTURAL)"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H259","v":{"v":0,"d":"0.00"}}]
[23138,"8.4.6.1",null,"Seal between concrete roof slabs and walls of chamber with approved Bitumen seal putty","m",{"v":20,"d":"20.00"},{"v":0,"d":"0.00"},{"$f":"IF(E265 = CHAR(37), F265*G265/100,F265*G265)","v":{"v":0,"d":"0.00"}}]
[]
[23174,"8.4.6.2",null,"Seal chamber base to wall construction joint on external face with approved 100mm wide bitumen waterproof bandage","m",{"v":15,"d":"15.00"},{"v":0,"d":"0.00"},{"$f":"IF(E267 = CHAR(37), F267*G267/100,F267*G267)","v":{"v":0,"d":"0.00"}}]
[]
[23192,"8.4.6.3",null,"Seal chamber wall to roof construction joint on external face with approved 100mm wide bitumen waterproof bandage","m",{"v":15,"d":"15.00"},{"v":0,"d":"0.00"},{"$f":"IF(E269 = CHAR(37), F269*G269/100,F269*G269)","v":{"v":0,"d":"0.00"}}]
[]
[23139,"8.4.6.4",null,"Plug 75mm-100mm dia lifting holes x 200mm deep in chamber roof slabs with approved Bitumen seal putty","No.",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"$f":"IF(E271 = CHAR(37), F271*G271/100,F271*G271)","v":{"v":0,"d":"0.00"}}]
[]
[23171,"8.4.7","SABS 1200L 8.2.13 ","PRECAST VALVE CHAMBERS AND MANHOLES"]
[]
[23172,null,null,"The following rates are to include for the supply and installation of all ladders, sealing joints, water proof bandaging joints, air vents, handrails, access manholes & frames, GRP landings, ladders & gratings, air vents and crushed stone. All in situ and pre-cast concrete, foundations, crushed stone layers, shuttering, surface finishing, curing of concrete and ancillaries to be included and rate supplied to be for complete functional unit. "]
[]
[23173,"8.4.7.1",null,"Supply and install Residue Meter Chambers COMPLETE with related items as per Dwg 60398/19, for depths up to 4,0m ","No.",{"v":8,"d":"8.00"},{"v":0,"d":"0.00"},{"$f":"IF(E277 = CHAR(37), F277*G277/100,F277*G277)","v":{"v":0,"d":"0.00"}}]
[]
[23188,"8.4.7.2",null,"Supply and install DN100 IV Chambers COMPLETE with related items as per Dwg 60398/17, for depths up to 4,0m ","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E279 = CHAR(37), F279*G279/100,F279*G279)","v":{"v":0,"d":"0.00"}}]
[]
[23130,"8.4.8",null,"CASTING IN"]
[]
[23128,null,null,"Supply all labour, plant and materials for casting of fabricated pipe specials into concrete walls of all thicknesses and wrapping with \"Denso 1250/300\" Tape wrapping system 600mm long to manufacturer's specifications (puddle flange not to be wrapped) inclusive for forming formwork around pipes and fixing pipes to the designated lines and levels, for:"]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H264:H284)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 8 - BACKWASH, SLUDGE AND BACKWASH RECOVERY SYSTEMS & "]
[null,"CHAMBERS"]
[{"$nulls":7},"SECTION 8.4: CONCRETE (STRUCTURAL)"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H285","v":{"v":0,"d":"0.00"}}]
[23169,"8.4.8.1",null,"up to DN300","No.",{"v":8,"d":"8.00"},{"v":0,"d":"0.00"},{"$f":"IF(E291 = CHAR(37), F291*G291/100,F291*G291)","v":{"v":0,"d":"0.00"}}]
[]
[23123,null,"PSG 8.10","Supply all labour, plant and materials for casting in, inclusive of forming formwork around items and fixing to the designated lines and levels, for:"]
[]
[23124,"8.4.8.2",null,"Air vents in chamber as per Detail on Dwg 60398/46","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E295 = CHAR(37), F295*G295/100,F295*G295)","v":{"v":0,"d":"0.00"}}]
[]
[23125,"8.4.8.3",null,"75mm-100mm dia lifting holes cast into roof slab as per detail on Dwg 60398/21","No.",{"v":16,"d":"16.00"},{"v":0,"d":"0.00"},{"$f":"IF(E297 = CHAR(37), F297*G297/100,F297*G297)","v":{"v":0,"d":"0.00"}}]
[]
[23129,"8.4.9",null,"MISCELLANEOUS"]
[]
[23152,null,null,"Supply all labour, plant and materials and wrap circumference of steel pipeline with \"Denso 1250/300\" Tape wrapping where ordered by the Engineer, for:"]
[]
[23153,"8.4.9.1",null,"up to DN300","m",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E303 = CHAR(37), F303*G303/100,F303*G303)","v":{"v":0,"d":"0.00"}}]
[]
[23140,"8.4.9.2",null,"Paint chamber roof slabs with 2 coats of white road marking paint including stenciling of chamber description in black","m²",{"v":15,"d":"15.00"},{"v":0,"d":"0.00"},{"$f":"IF(E305 = CHAR(37), F305*G305/100,F305*G305)","v":{"v":0,"d":"0.00"}}]
[]
[23149,"8.4.9.3",null,"Paint chamber walls where above ground with 2 coats of white road marking paint ","m²",{"v":30,"d":"30.00"},{"v":0,"d":"0.00"},{"$f":"IF(E307 = CHAR(37), F307*G307/100,F307*G307)","v":{"v":0,"d":"0.00"}}]
[]
[24202,"8.4.9.4",null,"Core through existing reinforced concrete wall for backwash recovery pipework, inclusive of grouting and waterproofing","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E309 = CHAR(37), F309*G309/100,F309*G309)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":21}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H290:H330)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 8 - BACKWASH, SLUDGE AND BACKWASH RECOVERY SYSTEMS & "]
[null,"CHAMBERS"]
[{"$nulls":7},"SECTION 8.5: MEDIUM PRESSURE PIPELINES (STEEL)"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[22479,"8.5","SABS 1200 L","MEDIUM PRESSURE PIPELINES (STEEL)"]
[]
[22480,"8.5.1","PSL 8.2.1","SUPPLY, LAY AND BED PIPE"]
[]
[22514,null,null,"Rate is inclusive of  checking for holidays of external coating and internal lining if applicable, jointing of pipe in accordance with the project specification, for:\r\n"]
[]
[22532,"8.5.1.1","PSL 8.2.1","DN100 to DN200 Steel 4.5mm thick X42","m",{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"$f":"IF(E342 = CHAR(37), F342*G342/100,F342*G342)","v":{"v":0,"d":"0.00"}}]
[]
[22478,"8.5.1.2","PSL 8.2.1","DN 250 to 400 Steel 4.5mm thick X42","m",{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"$f":"IF(E344 = CHAR(37), F344*G344/100,F344*G344)","v":{"v":0,"d":"0.00"}}]
[]
[22512,"8.5.2",null,"PREPARATION AND WELDING OF JOINTS IN X42 GRADE STEEL PIPE"]
[]
[22513,null,null,"Rate is inclusive NDT testing of joints and reinstatement at the joint for external coating and internal lining damage in accordance with the project specification."]
[]
[22481,null,"PSL 8.2.22","Preparation and welding of bell ended joint:"]
[]
[22482,"8.5.2.1",null,"DN100 to 400, 4.5mm thick","No.",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E352 = CHAR(37), F352*G352/100,F352*G352)","v":{"v":0,"d":"0.00"}}]
[]
[22506,null,"PSL 8.2.23","Preparation and welding of single mitred joints (Provisional):"]
[]
[22507,"8.5.2.2",null,"DN100 to 400, 4.5mm thick","No.",{"v":8,"d":"8.00"},{"v":0,"d":"0.00"},{"$f":"IF(E356 = CHAR(37), F356*G356/100,F356*G356)","v":{"v":0,"d":"0.00"}}]
[]
[22508,null,"PSL 8.2.24","Preparation and welding of collar/ band welded joints (Provisional):"]
[]
[22509,"8.5.2.3",null,"DN100 to 400, 4.5mm thick","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E360 = CHAR(37), F360*G360/100,F360*G360)","v":{"v":0,"d":"0.00"}}]
[]
[22510,null,"PSL 8.2.25","Preparation of X42 grade steel pipe by means of cutting where directed by the Engineer (provisional quantity):"]
[]
[22511,"8.5.2.4",null,"DN100 to 400, 4.5mm thick","No.",{"v":3,"d":"3.00"},{"v":0,"d":"0.00"},{"$f":"IF(E364 = CHAR(37), F364*G364/100,F364*G364)","v":{"v":0,"d":"0.00"}}]
[]
[22505,"8.5.3",null,"PIPE FITTINGS"]
[]
[22500,null,"PSL 8.2.2","Extra-over Item above for fabrication and installation of following specials: "]
[]
[22501,null,"PSL 3.4.4.2","Manufacturing of Simple and Compound Bends complete and install inclusive of cutting, welding, testing, reinstatement of external coating and internal lining, transportation and handling, for: "]
[]
[22515,null,null,"DN100 to 400, 4.5mm thick, X42, for:"]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H336:H372)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 8 - BACKWASH, SLUDGE AND BACKWASH RECOVERY SYSTEMS & "]
[null,"CHAMBERS"]
[{"$nulls":7},"SECTION 8.5: MEDIUM PRESSURE PIPELINES (STEEL)"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H373","v":{"v":0,"d":"0.00"}}]
[22516,"8.5.3.1",null,"greater than 0 to 15 deg","No.",{"v":3,"d":"3.00"},{"v":0,"d":"0.00"},{"$f":"IF(E379 = CHAR(37), F379*G379/100,F379*G379)","v":{"v":0,"d":"0.00"}}]
[]
[22517,"8.5.3.2",null,"greater than 15 to 30 deg ","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E381 = CHAR(37), F381*G381/100,F381*G381)","v":{"v":0,"d":"0.00"}}]
[]
[22518,"8.5.3.3",null,"greater than 30 to 45 deg ","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E383 = CHAR(37), F383*G383/100,F383*G383)","v":{"v":0,"d":"0.00"}}]
[]
[22519,"8.5.3.4",null,"greater than 45 to 60 deg ","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E385 = CHAR(37), F385*G385/100,F385*G385)","v":{"v":0,"d":"0.00"}}]
[]
[22520,"8.5.3.5",null,"greater than 60 to 75 deg ","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E387 = CHAR(37), F387*G387/100,F387*G387)","v":{"v":0,"d":"0.00"}}]
[]
[22521,"8.5.3.6",null,"greater than 75 to 90 deg ","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E389 = CHAR(37), F389*G389/100,F389*G389)","v":{"v":0,"d":"0.00"}}]
[]
[22522,"8.5.3.7","PSL 3.4.4.2","Supply Shop Drawings for fabricated steel segmented bends for approval","No.",{"v":13,"d":"13.00"},{"v":0,"d":"0.00"},{"$f":"IF(E391 = CHAR(37), F391*G391/100,F391*G391)","v":{"v":0,"d":"0.00"}}]
[]
[22483,null,null,"Supply and install the following steel slip on pipe flanges:"]
[]
[22484,null,null,"Rate to include cutting of pipes, joint preparation, welding, NDT testing of joints and reinstatement at the joint for external coating and internal lining damage complete in accordance with the project specification."]
[]
[22485,null,null,"SANS 1123 - Table 1600/3 (PN16):"]
[]
[22486,"8.5.3.8",null,"DN100 to 400, 4.5mm thick","No.",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E399 = CHAR(37), F399*G399/100,F399*G399)","v":{"v":0,"d":"0.00"}}]
[]
[22533,null,null,"Supply and install the following steel blank flanges:"]
[]
[22534,null,null,"SANS 1123 - Table 1600/3 (PN16):"]
[]
[22535,"8.5.3.9",null,"DN100 to 400, 4.5mm thick","No.",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E405 = CHAR(37), F405*G405/100,F405*G405)","v":{"v":0,"d":"0.00"}}]
[]
[22487,"8.5.4","PSL 3.9","REPAIR:"]
[]
[22488,null,null,"Repair, as result of damage inflicted by pipe supplier, external \"3 Layer Polyethylene\" coating complete inclusive of labour, materials, plant, supervision and QA/QC for defects:"]
[]
[22489,"8.5.4.1",null,"DN100 to 400, 4.5mm thick","m",{"v":60,"d":"60.00"},{"v":0,"d":"0.00"},{"$f":"IF(E411 = CHAR(37), F411*G411/100,F411*G411)","v":{"v":0,"d":"0.00"}}]
[]
[22490,"8.5.4.2",null,"from 501mm² to 750mm² in area","Prov No.",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E413 = CHAR(37), F413*G413/100,F413*G413)","v":{"v":0,"d":"0.00"}}]
[]
[22491,"8.5.4.3",null,"from 751m² to 1000mm² in area","Prov No.",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E415 = CHAR(37), F415*G415/100,F415*G415)","v":{"v":0,"d":"0.00"}}]
[]
[22492,"8.5.4.4",null,"from 1001mm² to 1400mm² in area","Prov No.",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E417 = CHAR(37), F417*G417/100,F417*G417)","v":{"v":0,"d":"0.00"}}]
[]
[]
[]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H378:H421)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 8 - BACKWASH, SLUDGE AND BACKWASH RECOVERY SYSTEMS & "]
[null,"CHAMBERS"]
[{"$nulls":7},"SECTION 8.5: MEDIUM PRESSURE PIPELINES (STEEL)"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H422","v":{"v":0,"d":"0.00"}}]
[22493,null,null,"Repair, as a result of damage inflicted by pipe supplier, internal cement mortar lining, complete inclusive of labour, plant, materials, supervision and QA/QC for defects for:"]
[]
[22494,"8.5.4.5",null,"up to 200mm² in area","Prov No.",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E430 = CHAR(37), F430*G430/100,F430*G430)","v":{"v":0,"d":"0.00"}}]
[]
[22495,"8.5.4.6",null,"from 201mm² to 400mm² in area","Prov No.",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E432 = CHAR(37), F432*G432/100,F432*G432)","v":{"v":0,"d":"0.00"}}]
[]
[22496,"8.5.4.7",null,"from 401mm² to 600mm² in area","Prov No.",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E434 = CHAR(37), F434*G434/100,F434*G434)","v":{"v":0,"d":"0.00"}}]
[]
[22497,"8.5.4.8",null,"from 600mm² to 800mm² in area","Prov No.",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E436 = CHAR(37), F436*G436/100,F436*G436)","v":{"v":0,"d":"0.00"}}]
[]
[22498,"8.5.4.9",null,"from 800mm² to 1000mm² in area","Prov No.",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E438 = CHAR(37), F438*G438/100,F438*G438)","v":{"v":0,"d":"0.00"}}]
[]
[22499,"8.5.4.10",null,"Repair inside lining and outside coating in terms of the specification, as a result of thermal welding conducted by employers corrosion specialist, to attach a monitoring cable to the crown of the pipe.","Prov No.",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E440 = CHAR(37), F440*G440/100,F440*G440)","v":{"v":0,"d":"0.00"}}]
[]
[22502,"8.5.5","PSL 7.3","HYDRAULIC TESTING "]
[]
[22503,null,"PSL 7.3 \r\nPSL 8.2.21","End cap, filling, testing and disinfection of pipelines inclusive of specials in chambers within sections as per specification, for:"]
[]
[22504,"8.5.5.1",null,"All diameter's of pipework when necessary","m",{"v":250,"d":"250.00"},{"v":0,"d":"0.00"},{"$f":"IF(E446 = CHAR(37), F446*G446/100,F446*G446)","v":{"v":0,"d":"0.00"}}]
[]
[22523,"8.5.6",null,"MISCELLANEOUS"]
[]
[22524,"8.5.6.1",null,"Cleaning of internal surfaces of pipeline where instructed by the Engineer","m",{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"$f":"IF(E450 = CHAR(37), F450*G450/100,F450*G450)","v":{"v":0,"d":"0.00"}}]
[]
[22525,null,null,"Supply all labour, plant and materials and install the following:"]
[]
[22526,"8.5.6.2",null,"Up to DN400 insulating flanges (inclusive of all sleeves and bolts)","No.",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E454 = CHAR(37), F454*G454/100,F454*G454)","v":{"v":0,"d":"0.00"}}]
[]
[22527,null,null,"Paint all above ground pipework as per specification with an approved UV stable overcoat"]
[]
[22528,"8.5.6.3",null,"Up to DN400","m",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E458 = CHAR(37), F458*G458/100,F458*G458)","v":{"v":0,"d":"0.00"}}]
[]
[22529,"8.5.7",null,"TIE INS"]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H427:H461)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 8 - BACKWASH, SLUDGE AND BACKWASH RECOVERY SYSTEMS & "]
[null,"CHAMBERS"]
[{"$nulls":7},"SECTION 8.5: MEDIUM PRESSURE PIPELINES (STEEL)"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H462","v":{"v":0,"d":"0.00"}}]
[22530,null,null,"Undertake the following tie-ins including the removal of sufficient existing pipe to make way for new pipework, arranging shut-downs with eThekwini Municipality operations staff, cleaning and preparing the pipes for cutting, removal of blank flange, dealing with all water (including that from leaking valves), preparing the pipe ends for jointing, re-commissioning the pipeline and making good on site including all temporary supports. (All new pipes, valves and fittings that are required are measured elsewhere), for:"]
[]
[22531,"8.5.7.1",null,"Metcalfe System","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E470 = CHAR(37), F470*G470/100,F470*G470)","v":{"v":0,"d":"0.00"}}]
[]
[23193,"8.5.7.2",null,"Tongaat South System","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E472 = CHAR(37), F472*G472/100,F472*G472)","v":{"v":0,"d":"0.00"}}]
[]
[23194,"8.5.7.3",null,"Hambanathi System","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E474 = CHAR(37), F474*G474/100,F474*G474)","v":{"v":0,"d":"0.00"}}]
[]
[23195,"8.5.7.4",null,"Mamba Ridge Back-feed system","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E476 = CHAR(37), F476*G476/100,F476*G476)","v":{"v":0,"d":"0.00"}}]
[]
[23196,"8.5.7.5",null,"Backwash Recovery System","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E478 = CHAR(37), F478*G478/100,F478*G478)","v":{"v":0,"d":"0.00"}}]
[]
[23197,"8.5.7.6",null,"Residue Disposal System","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E480 = CHAR(37), F480*G480/100,F480*G480)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":31}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H467:H511)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 8 - BACKWASH, SLUDGE AND BACKWASH RECOVERY SYSTEMS & "]
[null,"CHAMBERS"]
[{"$nulls":7},"SECTION 8.6: PIPEWORK ASSEMBLIES"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[22062,"8.6","SANS 1200 L, PSL","PIPEWORK ASSEMBLIES"]
[]
[23198,null,null,"Fabricate, supply and install valves, spool pieces, fittings and bends complete inclusive of all collar/ crotch plate reinforcing with internal and external coating as per specifications. Rates to include for all bolts, nuts, gaskets and jointing material, testing, holiday detection, radiographic inspection of field welds, preparation for welding where required and the repair and making good of all linings and coatings. All rates to be inclusive of UV protective coating where pipework is above ground."]
[]
[22108,"8.6.1","8.2.5 PSL 8.2.5","BLOWER PIPEWORK COMPLETE, PN16 UNLESS OTHERWISE STATED AS PER DWG 60398/03"]
[]
[22093,null,null,"All flanges to be supplied and as per SANS 1123 Table 1600/3 unless otherwise shown or specified "]
[]
[23979,"8.6.1.1",null,"Item A01","No.",{"v":3,"d":"3.00"},{"v":0,"d":"0.00"},{"$f":"IF(E525 = CHAR(37), F525*G525/100,F525*G525)","v":{"v":0,"d":"0.00"}}]
[]
[23980,"8.6.1.2",null,"Item A02","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E527 = CHAR(37), F527*G527/100,F527*G527)","v":{"v":0,"d":"0.00"}}]
[]
[23981,"8.6.1.3",null,"Item A03","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E529 = CHAR(37), F529*G529/100,F529*G529)","v":{"v":0,"d":"0.00"}}]
[]
[23982,"8.6.1.4",null,"Item A04","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E531 = CHAR(37), F531*G531/100,F531*G531)","v":{"v":0,"d":"0.00"}}]
[]
[23983,"8.6.1.5",null,"Item A05","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E533 = CHAR(37), F533*G533/100,F533*G533)","v":{"v":0,"d":"0.00"}}]
[]
[23984,"8.6.1.6",null,"Item A06","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E535 = CHAR(37), F535*G535/100,F535*G535)","v":{"v":0,"d":"0.00"}}]
[]
[23985,"8.6.1.7",null,"Item A07","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E537 = CHAR(37), F537*G537/100,F537*G537)","v":{"v":0,"d":"0.00"}}]
[]
[23986,"8.6.1.8",null,"Item A08","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E539 = CHAR(37), F539*G539/100,F539*G539)","v":{"v":0,"d":"0.00"}}]
[]
[23987,"8.6.1.9",null,"Item A09","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E541 = CHAR(37), F541*G541/100,F541*G541)","v":{"v":0,"d":"0.00"}}]
[]
[23988,"8.6.1.10",null,"Item A10","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E543 = CHAR(37), F543*G543/100,F543*G543)","v":{"v":0,"d":"0.00"}}]
[]
[23989,"8.6.1.11",null,"Item A11","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E545 = CHAR(37), F545*G545/100,F545*G545)","v":{"v":0,"d":"0.00"}}]
[]
[23990,"8.6.1.12",null,"Item A12","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E547 = CHAR(37), F547*G547/100,F547*G547)","v":{"v":0,"d":"0.00"}}]
[]
[23991,"8.6.1.13",null,"Item A13","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E549 = CHAR(37), F549*G549/100,F549*G549)","v":{"v":0,"d":"0.00"}}]
[]
[23992,"8.6.1.14",null,"Item A14","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E551 = CHAR(37), F551*G551/100,F551*G551)","v":{"v":0,"d":"0.00"}}]
[]
[23993,"8.6.1.15",null,"Item A15","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E553 = CHAR(37), F553*G553/100,F553*G553)","v":{"v":0,"d":"0.00"}}]
[]
[23994,"8.6.1.16",null,"Item A16","No.",{"v":14,"d":"14.00"},{"v":0,"d":"0.00"},{"$f":"IF(E555 = CHAR(37), F555*G555/100,F555*G555)","v":{"v":0,"d":"0.00"}}]
[]
[23995,"8.6.1.17",null,"Item A17","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E557 = CHAR(37), F557*G557/100,F557*G557)","v":{"v":0,"d":"0.00"}}]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H517:H558)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 8 - BACKWASH, SLUDGE AND BACKWASH RECOVERY SYSTEMS & "]
[null,"CHAMBERS"]
[{"$nulls":7},"SECTION 8.6: PIPEWORK ASSEMBLIES"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H559","v":{"v":0,"d":"0.00"}}]
[23996,"8.6.1.18",null,"Item A18","No.",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E565 = CHAR(37), F565*G565/100,F565*G565)","v":{"v":0,"d":"0.00"}}]
[]
[23997,"8.6.1.19",null,"Item A19","No.",{"v":6,"d":"6.00"},{"v":0,"d":"0.00"},{"$f":"IF(E567 = CHAR(37), F567*G567/100,F567*G567)","v":{"v":0,"d":"0.00"}}]
[]
[23998,"8.6.1.20",null,"Item A20","No.",{"v":6,"d":"6.00"},{"v":0,"d":"0.00"},{"$f":"IF(E569 = CHAR(37), F569*G569/100,F569*G569)","v":{"v":0,"d":"0.00"}}]
[]
[23999,"8.6.1.21",null,"Item A21","No.",{"v":6,"d":"6.00"},{"v":0,"d":"0.00"},{"$f":"IF(E571 = CHAR(37), F571*G571/100,F571*G571)","v":{"v":0,"d":"0.00"}}]
[]
[24000,"8.6.1.22",null,"Item A22","No.",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E573 = CHAR(37), F573*G573/100,F573*G573)","v":{"v":0,"d":"0.00"}}]
[]
[24001,"8.6.1.23",null,"Item A23","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E575 = CHAR(37), F575*G575/100,F575*G575)","v":{"v":0,"d":"0.00"}}]
[]
[24071,"8.6.2","8.2.5 PSL 8.2.5","BACKWASH RECOVERY ASSEMBLY COMPLETE, PN16 UNLESS OTHERWISE STATED AS PER DWG 60398/05"]
[]
[24072,null,null,"All flanges to be supplied and as per SANS 1123 Table 1600/3 unless otherwise shown or specified "]
[]
[24002,"8.6.2.1",null,"Item B01","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E581 = CHAR(37), F581*G581/100,F581*G581)","v":{"v":0,"d":"0.00"}}]
[]
[24003,"8.6.2.2",null,"Item B02","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E583 = CHAR(37), F583*G583/100,F583*G583)","v":{"v":0,"d":"0.00"}}]
[]
[24004,"8.6.2.3",null,"Item B03","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E585 = CHAR(37), F585*G585/100,F585*G585)","v":{"v":0,"d":"0.00"}}]
[]
[24005,"8.6.2.4",null,"Item B04","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E587 = CHAR(37), F587*G587/100,F587*G587)","v":{"v":0,"d":"0.00"}}]
[]
[24006,"8.6.2.5",null,"Item B05","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E589 = CHAR(37), F589*G589/100,F589*G589)","v":{"v":0,"d":"0.00"}}]
[]
[24007,"8.6.2.6",null,"Item B06","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E591 = CHAR(37), F591*G591/100,F591*G591)","v":{"v":0,"d":"0.00"}}]
[]
[24008,"8.6.2.7",null,"Item B07","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E593 = CHAR(37), F593*G593/100,F593*G593)","v":{"v":0,"d":"0.00"}}]
[]
[24009,"8.6.2.8",null,"Item B08","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E595 = CHAR(37), F595*G595/100,F595*G595)","v":{"v":0,"d":"0.00"}}]
[]
[24010,"8.6.2.9",null,"Item B09","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E597 = CHAR(37), F597*G597/100,F597*G597)","v":{"v":0,"d":"0.00"}}]
[]
[24011,"8.6.2.10",null,"Item B10","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E599 = CHAR(37), F599*G599/100,F599*G599)","v":{"v":0,"d":"0.00"}}]
[]
[24012,"8.6.2.11",null,"Item B11","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E601 = CHAR(37), F601*G601/100,F601*G601)","v":{"v":0,"d":"0.00"}}]
[]
[24013,"8.6.2.12",null,"Item B12","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E603 = CHAR(37), F603*G603/100,F603*G603)","v":{"v":0,"d":"0.00"}}]
[]
[24014,"8.6.2.13",null,"Item B13","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E605 = CHAR(37), F605*G605/100,F605*G605)","v":{"v":0,"d":"0.00"}}]
[]
[24015,"8.6.2.14",null,"Item B14","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E607 = CHAR(37), F607*G607/100,F607*G607)","v":{"v":0,"d":"0.00"}}]
[]
[24016,"8.6.2.15",null,"Item B15","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E609 = CHAR(37), F609*G609/100,F609*G609)","v":{"v":0,"d":"0.00"}}]
[]
[24017,"8.6.2.16",null,"Item B16","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E611 = CHAR(37), F611*G611/100,F611*G611)","v":{"v":0,"d":"0.00"}}]
[]
[24018,"8.6.2.17",null,"Item B17","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E613 = CHAR(37), F613*G613/100,F613*G613)","v":{"v":0,"d":"0.00"}}]
[]
[24019,"8.6.2.18",null,"Item B18","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E615 = CHAR(37), F615*G615/100,F615*G615)","v":{"v":0,"d":"0.00"}}]
[]
[24020,"8.6.2.19",null,"Item B19","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E617 = CHAR(37), F617*G617/100,F617*G617)","v":{"v":0,"d":"0.00"}}]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H564:H617)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 8 - BACKWASH, SLUDGE AND BACKWASH RECOVERY SYSTEMS & "]
[null,"CHAMBERS"]
[{"$nulls":7},"SECTION 8.6: PIPEWORK ASSEMBLIES"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H618","v":{"v":0,"d":"0.00"}}]
[24021,"8.6.2.20",null,"Item B20","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E624 = CHAR(37), F624*G624/100,F624*G624)","v":{"v":0,"d":"0.00"}}]
[]
[24073,"8.6.3","8.2.5 PSL 8.2.5","BACKWASH PIPEWORK ASSEMBLY COMPLETE, PN16 UNLESS OTHERWISE STATED AS PER DWG 60398/04"]
[]
[24074,null,null,"All flanges to be supplied and as per SANS 1123 Table 1600/3 unless otherwise shown or specified "]
[]
[24022,"8.6.3.1",null,"Item D01","No.",{"v":3,"d":"3.00"},{"v":0,"d":"0.00"},{"$f":"IF(E630 = CHAR(37), F630*G630/100,F630*G630)","v":{"v":0,"d":"0.00"}}]
[]
[24023,"8.6.3.2",null,"Item D02","No.",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"$f":"IF(E632 = CHAR(37), F632*G632/100,F632*G632)","v":{"v":0,"d":"0.00"}}]
[]
[24024,"8.6.3.3",null,"Item D03","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E634 = CHAR(37), F634*G634/100,F634*G634)","v":{"v":0,"d":"0.00"}}]
[]
[24025,"8.6.3.4",null,"Item D04","No.",{"v":3,"d":"3.00"},{"v":0,"d":"0.00"},{"$f":"IF(E636 = CHAR(37), F636*G636/100,F636*G636)","v":{"v":0,"d":"0.00"}}]
[]
[24026,"8.6.3.5",null,"Item D05","No.",{"v":3,"d":"3.00"},{"v":0,"d":"0.00"},{"$f":"IF(E638 = CHAR(37), F638*G638/100,F638*G638)","v":{"v":0,"d":"0.00"}}]
[]
[24027,"8.6.3.6",null,"Item D06","No.",{"v":3,"d":"3.00"},{"v":0,"d":"0.00"},{"$f":"IF(E640 = CHAR(37), F640*G640/100,F640*G640)","v":{"v":0,"d":"0.00"}}]
[]
[24028,"8.6.3.7",null,"Item D07","No.",{"v":3,"d":"3.00"},{"v":0,"d":"0.00"},{"$f":"IF(E642 = CHAR(37), F642*G642/100,F642*G642)","v":{"v":0,"d":"0.00"}}]
[]
[24029,"8.6.3.8",null,"Item D08","No.",{"v":3,"d":"3.00"},{"v":0,"d":"0.00"},{"$f":"IF(E644 = CHAR(37), F644*G644/100,F644*G644)","v":{"v":0,"d":"0.00"}}]
[]
[24030,"8.6.3.9",null,"Item D09","No.",{"v":3,"d":"3.00"},{"v":0,"d":"0.00"},{"$f":"IF(E646 = CHAR(37), F646*G646/100,F646*G646)","v":{"v":0,"d":"0.00"}}]
[]
[24031,"8.6.3.10",null,"Item D10","No.",{"v":3,"d":"3.00"},{"v":0,"d":"0.00"},{"$f":"IF(E648 = CHAR(37), F648*G648/100,F648*G648)","v":{"v":0,"d":"0.00"}}]
[]
[24032,"8.6.3.11",null,"Item D11","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E650 = CHAR(37), F650*G650/100,F650*G650)","v":{"v":0,"d":"0.00"}}]
[]
[24033,"8.6.3.12",null,"Item D12","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E652 = CHAR(37), F652*G652/100,F652*G652)","v":{"v":0,"d":"0.00"}}]
[]
[24034,"8.6.3.13",null,"Item D13","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E654 = CHAR(37), F654*G654/100,F654*G654)","v":{"v":0,"d":"0.00"}}]
[]
[24035,"8.6.3.14",null,"Item D14","No.",{"v":7,"d":"7.00"},{"v":0,"d":"0.00"},{"$f":"IF(E656 = CHAR(37), F656*G656/100,F656*G656)","v":{"v":0,"d":"0.00"}}]
[]
[24036,"8.6.3.15",null,"Item D15","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E658 = CHAR(37), F658*G658/100,F658*G658)","v":{"v":0,"d":"0.00"}}]
[]
[24037,"8.6.3.16",null,"Item D16","No.",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"$f":"IF(E660 = CHAR(37), F660*G660/100,F660*G660)","v":{"v":0,"d":"0.00"}}]
[]
[24038,"8.6.3.17",null,"Item D17","No.",{"v":3,"d":"3.00"},{"v":0,"d":"0.00"},{"$f":"IF(E662 = CHAR(37), F662*G662/100,F662*G662)","v":{"v":0,"d":"0.00"}}]
[]
[24039,"8.6.3.18",null,"Item D18","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E664 = CHAR(37), F664*G664/100,F664*G664)","v":{"v":0,"d":"0.00"}}]
[]
[24040,"8.6.3.19",null,"Item D19","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E666 = CHAR(37), F666*G666/100,F666*G666)","v":{"v":0,"d":"0.00"}}]
[]
[24041,"8.6.3.20",null,"Item D20","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E668 = CHAR(37), F668*G668/100,F668*G668)","v":{"v":0,"d":"0.00"}}]
[]
[24042,"8.6.3.21",null,"Item D22","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E670 = CHAR(37), F670*G670/100,F670*G670)","v":{"v":0,"d":"0.00"}}]
[]
[24043,"8.6.3.22",null,"Item D23","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E672 = CHAR(37), F672*G672/100,F672*G672)","v":{"v":0,"d":"0.00"}}]
[]
[24044,"8.6.3.23",null,"Item D24","No.",{"v":6,"d":"6.00"},{"v":0,"d":"0.00"},{"$f":"IF(E674 = CHAR(37), F674*G674/100,F674*G674)","v":{"v":0,"d":"0.00"}}]
[]
[24045,"8.6.3.24",null,"Item D25","No.",{"v":6,"d":"6.00"},{"v":0,"d":"0.00"},{"$f":"IF(E676 = CHAR(37), F676*G676/100,F676*G676)","v":{"v":0,"d":"0.00"}}]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H623:H676)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 8 - BACKWASH, SLUDGE AND BACKWASH RECOVERY SYSTEMS & "]
[null,"CHAMBERS"]
[{"$nulls":7},"SECTION 8.6: PIPEWORK ASSEMBLIES"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H677","v":{"v":0,"d":"0.00"}}]
[24046,"8.6.3.25",null,"Item D26","No.",{"v":6,"d":"6.00"},{"v":0,"d":"0.00"},{"$f":"IF(E683 = CHAR(37), F683*G683/100,F683*G683)","v":{"v":0,"d":"0.00"}}]
[]
[24047,"8.6.3.26",null,"Item D27","No.",{"v":6,"d":"6.00"},{"v":0,"d":"0.00"},{"$f":"IF(E685 = CHAR(37), F685*G685/100,F685*G685)","v":{"v":0,"d":"0.00"}}]
[]
[24048,"8.6.3.27",null,"Item D28","No.",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E687 = CHAR(37), F687*G687/100,F687*G687)","v":{"v":0,"d":"0.00"}}]
[]
[24049,"8.6.3.28",null,"Item D29","No.",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E689 = CHAR(37), F689*G689/100,F689*G689)","v":{"v":0,"d":"0.00"}}]
[]
[24050,"8.6.3.29",null,"Item D30","No.",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E691 = CHAR(37), F691*G691/100,F691*G691)","v":{"v":0,"d":"0.00"}}]
[]
[24051,"8.6.3.30",null,"Item D31","No.",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E693 = CHAR(37), F693*G693/100,F693*G693)","v":{"v":0,"d":"0.00"}}]
[]
[24052,"8.6.3.31",null,"Item D32","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E695 = CHAR(37), F695*G695/100,F695*G695)","v":{"v":0,"d":"0.00"}}]
[]
[24053,"8.6.3.32",null,"Item D33","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E697 = CHAR(37), F697*G697/100,F697*G697)","v":{"v":0,"d":"0.00"}}]
[]
[24054,"8.6.3.33",null,"Item D34","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E699 = CHAR(37), F699*G699/100,F699*G699)","v":{"v":0,"d":"0.00"}}]
[]
[24055,"8.6.3.34",null,"Item D35","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E701 = CHAR(37), F701*G701/100,F701*G701)","v":{"v":0,"d":"0.00"}}]
[]
[24056,"8.6.3.35",null,"Item D36","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E703 = CHAR(37), F703*G703/100,F703*G703)","v":{"v":0,"d":"0.00"}}]
[]
[24057,"8.6.3.36",null,"Item D37","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E705 = CHAR(37), F705*G705/100,F705*G705)","v":{"v":0,"d":"0.00"}}]
[]
[24058,"8.6.3.37",null,"Item D38","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E707 = CHAR(37), F707*G707/100,F707*G707)","v":{"v":0,"d":"0.00"}}]
[]
[24059,"8.6.3.38",null,"Item D39","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E709 = CHAR(37), F709*G709/100,F709*G709)","v":{"v":0,"d":"0.00"}}]
[]
[24060,"8.6.3.39",null,"Item D40","No.",{"v":12,"d":"12.00"},{"v":0,"d":"0.00"},{"$f":"IF(E711 = CHAR(37), F711*G711/100,F711*G711)","v":{"v":0,"d":"0.00"}}]
[]
[24061,"8.6.3.40",null,"Item D41","No.",{"v":12,"d":"12.00"},{"v":0,"d":"0.00"},{"$f":"IF(E713 = CHAR(37), F713*G713/100,F713*G713)","v":{"v":0,"d":"0.00"}}]
[]
[24062,"8.6.3.41",null,"Item D42","No.",{"v":23,"d":"23.00"},{"v":0,"d":"0.00"},{"$f":"IF(E715 = CHAR(37), F715*G715/100,F715*G715)","v":{"v":0,"d":"0.00"}}]
[]
[24063,"8.6.3.42",null,"Item D43","No.",{"v":12,"d":"12.00"},{"v":0,"d":"0.00"},{"$f":"IF(E717 = CHAR(37), F717*G717/100,F717*G717)","v":{"v":0,"d":"0.00"}}]
[]
[24064,"8.6.3.43",null,"Item D44","No.",{"v":12,"d":"12.00"},{"v":0,"d":"0.00"},{"$f":"IF(E719 = CHAR(37), F719*G719/100,F719*G719)","v":{"v":0,"d":"0.00"}}]
[]
[24065,"8.6.3.44",null,"Item D45","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E721 = CHAR(37), F721*G721/100,F721*G721)","v":{"v":0,"d":"0.00"}}]
[]
[24066,"8.6.3.45",null,"Item D46","No.",{"v":7,"d":"7.00"},{"v":0,"d":"0.00"},{"$f":"IF(E723 = CHAR(37), F723*G723/100,F723*G723)","v":{"v":0,"d":"0.00"}}]
[]
[24067,"8.6.3.46",null,"Item D47","No.",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"$f":"IF(E725 = CHAR(37), F725*G725/100,F725*G725)","v":{"v":0,"d":"0.00"}}]
[]
[24068,"8.6.3.47",null,"Item D48","No.",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"$f":"IF(E727 = CHAR(37), F727*G727/100,F727*G727)","v":{"v":0,"d":"0.00"}}]
[]
[24069,"8.6.3.48",null,"Item D49","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E729 = CHAR(37), F729*G729/100,F729*G729)","v":{"v":0,"d":"0.00"}}]
[]
[24070,"8.6.3.49",null,"Item D50","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E731 = CHAR(37), F731*G731/100,F731*G731)","v":{"v":0,"d":"0.00"}}]
[]
[24075,"8.6.4","8.2.5 PSL 8.2.5","DN250 ISOLATION VALVE CHAMBER ASSEMBLY COMPLETE, PN16 UNLESS OTHERWISE STATED AS PER DWG 60398/06"]
[]
[24076,null,null,"All flanges to be supplied and as per SANS 1123 Table 1600/3 unless otherwise shown or specified "]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H682:H735)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 8 - BACKWASH, SLUDGE AND BACKWASH RECOVERY SYSTEMS & "]
[null,"CHAMBERS"]
[{"$nulls":7},"SECTION 8.6: PIPEWORK ASSEMBLIES"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H736","v":{"v":0,"d":"0.00"}}]
[24077,"8.6.4.1",null,"Item 1","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E742 = CHAR(37), F742*G742/100,F742*G742)","v":{"v":0,"d":"0.00"}}]
[]
[24078,"8.6.4.2",null,"Item 2","No.",{"v":3,"d":"3.00"},{"v":0,"d":"0.00"},{"$f":"IF(E744 = CHAR(37), F744*G744/100,F744*G744)","v":{"v":0,"d":"0.00"}}]
[]
[24079,"8.6.4.3",null,"Item 3","No.",{"v":3,"d":"3.00"},{"v":0,"d":"0.00"},{"$f":"IF(E746 = CHAR(37), F746*G746/100,F746*G746)","v":{"v":0,"d":"0.00"}}]
[]
[24080,"8.6.4.4",null,"Item 4","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E748 = CHAR(37), F748*G748/100,F748*G748)","v":{"v":0,"d":"0.00"}}]
[]
[24081,"8.6.4.5",null,"Item 5","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E750 = CHAR(37), F750*G750/100,F750*G750)","v":{"v":0,"d":"0.00"}}]
[]
[24082,"8.6.4.6",null,"Item 6","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E752 = CHAR(37), F752*G752/100,F752*G752)","v":{"v":0,"d":"0.00"}}]
[]
[24083,"8.6.4.7",null,"Item 7","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E754 = CHAR(37), F754*G754/100,F754*G754)","v":{"v":0,"d":"0.00"}}]
[]
[24084,"8.6.4.8",null,"Item 8","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E756 = CHAR(37), F756*G756/100,F756*G756)","v":{"v":0,"d":"0.00"}}]
[]
[24085,"8.6.4.9",null,"Item 9","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E758 = CHAR(37), F758*G758/100,F758*G758)","v":{"v":0,"d":"0.00"}}]
[]
[24086,"8.6.4.10",null,"Item 10","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E760 = CHAR(37), F760*G760/100,F760*G760)","v":{"v":0,"d":"0.00"}}]
[]
[24087,"8.6.4.11",null,"Item 11","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E762 = CHAR(37), F762*G762/100,F762*G762)","v":{"v":0,"d":"0.00"}}]
[]
[24088,"8.6.4.12",null,"Item 12","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E764 = CHAR(37), F764*G764/100,F764*G764)","v":{"v":0,"d":"0.00"}}]
[]
[24089,"8.6.4.13",null,"Item 13","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E766 = CHAR(37), F766*G766/100,F766*G766)","v":{"v":0,"d":"0.00"}}]
[]
[24090,"8.6.4.14",null,"Item 14","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E768 = CHAR(37), F768*G768/100,F768*G768)","v":{"v":0,"d":"0.00"}}]
[]
[24091,"8.6.4.15",null,"Item 15","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E770 = CHAR(37), F770*G770/100,F770*G770)","v":{"v":0,"d":"0.00"}}]
[]
[24092,"8.6.4.16",null,"Item 16","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E772 = CHAR(37), F772*G772/100,F772*G772)","v":{"v":0,"d":"0.00"}}]
[]
[24093,"8.6.4.17",null,"Item 17","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E774 = CHAR(37), F774*G774/100,F774*G774)","v":{"v":0,"d":"0.00"}}]
[]
[24094,"8.6.4.18",null,"Item 18","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E776 = CHAR(37), F776*G776/100,F776*G776)","v":{"v":0,"d":"0.00"}}]
[]
[24095,"8.6.4.19",null,"Item 19","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E778 = CHAR(37), F778*G778/100,F778*G778)","v":{"v":0,"d":"0.00"}}]
[]
[24096,"8.6.4.20",null,"Item 20","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E780 = CHAR(37), F780*G780/100,F780*G780)","v":{"v":0,"d":"0.00"}}]
[]
[24097,"8.6.4.21",null,"Item 21","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E782 = CHAR(37), F782*G782/100,F782*G782)","v":{"v":0,"d":"0.00"}}]
[]
[24098,"8.6.4.22",null,"Item 22","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E784 = CHAR(37), F784*G784/100,F784*G784)","v":{"v":0,"d":"0.00"}}]
[]
[24099,"8.6.5","8.2.5 PSL 8.2.5","RESIDUE DISPOSAL SYSTEM ASSEMBLY COMPLETE, PN16 UNLESS OTHERWISE STATED AS PER DWG 60398/08"]
[]
[24100,null,null,"All flanges to be supplied and as per SANS 1123 Table 1600/3 unless otherwise shown or specified "]
[]
[24101,"8.6.5.1",null,"Item 1","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E790 = CHAR(37), F790*G790/100,F790*G790)","v":{"v":0,"d":"0.00"}}]
[]
[24102,"8.6.5.2",null,"Item 2","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E792 = CHAR(37), F792*G792/100,F792*G792)","v":{"v":0,"d":"0.00"}}]
[]
[24103,"8.6.5.3",null,"Item 3","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E794 = CHAR(37), F794*G794/100,F794*G794)","v":{"v":0,"d":"0.00"}}]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H741:H794)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 8 - BACKWASH, SLUDGE AND BACKWASH RECOVERY SYSTEMS & "]
[null,"CHAMBERS"]
[{"$nulls":7},"SECTION 8.6: PIPEWORK ASSEMBLIES"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H795","v":{"v":0,"d":"0.00"}}]
[24104,"8.6.5.4",null,"Item 4","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E801 = CHAR(37), F801*G801/100,F801*G801)","v":{"v":0,"d":"0.00"}}]
[]
[24105,"8.6.5.5",null,"Item 5","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E803 = CHAR(37), F803*G803/100,F803*G803)","v":{"v":0,"d":"0.00"}}]
[]
[24106,"8.6.5.6",null,"Item 6","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E805 = CHAR(37), F805*G805/100,F805*G805)","v":{"v":0,"d":"0.00"}}]
[]
[24107,"8.6.5.7",null,"Item 7","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E807 = CHAR(37), F807*G807/100,F807*G807)","v":{"v":0,"d":"0.00"}}]
[]
[24108,"8.6.5.8",null,"Item 8","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E809 = CHAR(37), F809*G809/100,F809*G809)","v":{"v":0,"d":"0.00"}}]
[]
[24109,"8.6.5.9",null,"Item 9","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E811 = CHAR(37), F811*G811/100,F811*G811)","v":{"v":0,"d":"0.00"}}]
[]
[24110,"8.6.5.10",null,"Item 10","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E813 = CHAR(37), F813*G813/100,F813*G813)","v":{"v":0,"d":"0.00"}}]
[]
[24111,"8.6.5.11",null,"Item 11","No.",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"$f":"IF(E815 = CHAR(37), F815*G815/100,F815*G815)","v":{"v":0,"d":"0.00"}}]
[]
[24112,"8.6.5.12",null,"Item 12","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E817 = CHAR(37), F817*G817/100,F817*G817)","v":{"v":0,"d":"0.00"}}]
[]
[24113,"8.6.5.13",null,"Item 13","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E819 = CHAR(37), F819*G819/100,F819*G819)","v":{"v":0,"d":"0.00"}}]
[]
[24114,"8.6.5.14",null,"Item 14","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E821 = CHAR(37), F821*G821/100,F821*G821)","v":{"v":0,"d":"0.00"}}]
[]
[24115,"8.6.5.15",null,"Item 15","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E823 = CHAR(37), F823*G823/100,F823*G823)","v":{"v":0,"d":"0.00"}}]
[]
[24116,"8.6.5.16",null,"Item 16","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E825 = CHAR(37), F825*G825/100,F825*G825)","v":{"v":0,"d":"0.00"}}]
[]
[24117,"8.6.5.17",null,"Item 17","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E827 = CHAR(37), F827*G827/100,F827*G827)","v":{"v":0,"d":"0.00"}}]
[]
[24118,"8.6.5.18",null,"Item 18","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E829 = CHAR(37), F829*G829/100,F829*G829)","v":{"v":0,"d":"0.00"}}]
[]
[24119,"8.6.5.19",null,"Item 19","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E831 = CHAR(37), F831*G831/100,F831*G831)","v":{"v":0,"d":"0.00"}}]
[]
[24120,"8.6.5.20",null,"Item 20","No.",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"$f":"IF(E833 = CHAR(37), F833*G833/100,F833*G833)","v":{"v":0,"d":"0.00"}}]
[]
[24121,"8.6.5.21",null,"Item 21","No.",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"$f":"IF(E835 = CHAR(37), F835*G835/100,F835*G835)","v":{"v":0,"d":"0.00"}}]
[]
[24122,"8.6.5.22",null,"Item 22","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E837 = CHAR(37), F837*G837/100,F837*G837)","v":{"v":0,"d":"0.00"}}]
[]
[24123,"8.6.5.23",null,"Item 23","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E839 = CHAR(37), F839*G839/100,F839*G839)","v":{"v":0,"d":"0.00"}}]
[]
[24124,"8.6.5.24",null,"Item 24","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E841 = CHAR(37), F841*G841/100,F841*G841)","v":{"v":0,"d":"0.00"}}]
[]
[24125,"8.6.5.25",null,"Item 25","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E843 = CHAR(37), F843*G843/100,F843*G843)","v":{"v":0,"d":"0.00"}}]
[]
[24126,"8.6.5.26",null,"Item 26","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E845 = CHAR(37), F845*G845/100,F845*G845)","v":{"v":0,"d":"0.00"}}]
[]
[24127,"8.6.5.27",null,"Item 27","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E847 = CHAR(37), F847*G847/100,F847*G847)","v":{"v":0,"d":"0.00"}}]
[]
[24128,"8.6.5.28",null,"Item 28","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E849 = CHAR(37), F849*G849/100,F849*G849)","v":{"v":0,"d":"0.00"}}]
[]
[24129,"8.6.6","8.2.5 PSL 8.2.5","DN100 ISOLATION VALVE (RESIDUE DISPOSAL AND BACKWASH RECOVERY CROSS CONNECTION) ASSEMBLY COMPLETE, PN16 UNLESS OTHERWISE STATED AS PER DWG 60398/07"]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H800:H852)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 8 - BACKWASH, SLUDGE AND BACKWASH RECOVERY SYSTEMS & "]
[null,"CHAMBERS"]
[{"$nulls":7},"SECTION 8.6: PIPEWORK ASSEMBLIES"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H853","v":{"v":0,"d":"0.00"}}]
[24130,null,null,"All flanges to be supplied and as per SANS 1123 Table 1600/3 unless otherwise shown or specified "]
[]
[24131,"8.6.6.1",null,"Item 1","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E861 = CHAR(37), F861*G861/100,F861*G861)","v":{"v":0,"d":"0.00"}}]
[]
[24132,"8.6.6.2",null,"Item 2","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E863 = CHAR(37), F863*G863/100,F863*G863)","v":{"v":0,"d":"0.00"}}]
[]
[24133,"8.6.6.3",null,"Item 3","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E865 = CHAR(37), F865*G865/100,F865*G865)","v":{"v":0,"d":"0.00"}}]
[]
[24134,"8.6.6.4",null,"Item 4","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E867 = CHAR(37), F867*G867/100,F867*G867)","v":{"v":0,"d":"0.00"}}]
[]
[24135,"8.6.6.5",null,"Item 5","No.",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"$f":"IF(E869 = CHAR(37), F869*G869/100,F869*G869)","v":{"v":0,"d":"0.00"}}]
[]
[24136,"8.6.6.6",null,"Item 6","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E871 = CHAR(37), F871*G871/100,F871*G871)","v":{"v":0,"d":"0.00"}}]
[]
[24137,"8.6.6.7",null,"Item 7","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E873 = CHAR(37), F873*G873/100,F873*G873)","v":{"v":0,"d":"0.00"}}]
[]
[24138,"8.6.6.8",null,"Item 8","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E875 = CHAR(37), F875*G875/100,F875*G875)","v":{"v":0,"d":"0.00"}}]
[]
[24139,"8.6.6.9",null,"Item 9","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E877 = CHAR(37), F877*G877/100,F877*G877)","v":{"v":0,"d":"0.00"}}]
[]
[24140,"8.6.6.10",null,"Item 10","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E879 = CHAR(37), F879*G879/100,F879*G879)","v":{"v":0,"d":"0.00"}}]
[]
[24141,"8.6.6.11",null,"Item 11","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E881 = CHAR(37), F881*G881/100,F881*G881)","v":{"v":0,"d":"0.00"}}]
[]
[24142,"8.6.6.12",null,"Item 12","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E883 = CHAR(37), F883*G883/100,F883*G883)","v":{"v":0,"d":"0.00"}}]
[]
[24143,"8.6.6.13",null,"Item 13","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E885 = CHAR(37), F885*G885/100,F885*G885)","v":{"v":0,"d":"0.00"}}]
[]
[24144,"8.6.6.14",null,"Item 14","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E887 = CHAR(37), F887*G887/100,F887*G887)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":27}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H858:H914)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 8 - BACKWASH, SLUDGE AND BACKWASH RECOVERY SYSTEMS & "]
[null,"CHAMBERS"]
[{"$nulls":7},"SECTION 8.7: BEDDING"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[22557,"8.7","SABS 1200 LB","BEDDING (PIPES)"]
[]
[22565,"8.7.1","PSLB 8.2.1","Provision of bedding from trench excavations:"]
[]
[22558,"8.7.1.1",null,"Selected granular material for 200mm bedding cradle below pipe invert","m³",{"v":30,"d":"30.00"},{"v":0,"d":"0.00"},{"$f":"IF(E924 = CHAR(37), F924*G924/100,F924*G924)","v":{"v":0,"d":"0.00"}}]
[]
[22559,"8.7.1.2",null,"Selected granular material for fill blanket to 300mm above pipe crown","m³",{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"$f":"IF(E926 = CHAR(37), F926*G926/100,F926*G926)","v":{"v":0,"d":"0.00"}}]
[]
[22561,"8.7.1.3","PSLB 8.2.1.1","Extra Over for screening of material from the trench excavation, to achieve grading suitable to comply with the bedding and blanket material specification (Provisional Quantity) ","m³",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E928 = CHAR(37), F928*G928/100,F928*G928)","v":{"v":0,"d":"0.00"}}]
[]
[22562,"8.7.2","PSLB 8.2.2","Supply only of bedding by importation:"]
[]
[22563,null,"PSLB 8.2.2.3","From commercial sources:"]
[]
[22564,"8.7.2.1",null,"a) Selected granular material for 200mm bedding cradle below pipe invert","m³",{"v":30,"d":"30.00"},{"v":0,"d":"0.00"},{"$f":"IF(E934 = CHAR(37), F934*G934/100,F934*G934)","v":{"v":0,"d":"0.00"}}]
[]
[22560,"8.7.2.2",null,"b) Selected granular material for fill blanket to 300mm above pipe crown","m³",{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"$f":"IF(E936 = CHAR(37), F936*G936/100,F936*G936)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":33}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H920:H969)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 8 - BACKWASH, SLUDGE AND BACKWASH RECOVERY SYSTEMS & "]
[null,"CHAMBERS"]
[{"$nulls":7},"SECTION 8.8: STRUCTURAL STEELWORK (SUNDRY ITEMS) AND GRP"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[23205,"8.8","SABS 1200 HA\r\nPSHA","STRUCTURAL STEELWORK (SUNDRY ITEMS) AND GRP"]
[]
[23214,"8.8.1",null,"ACCESS LADDERS AND LANDINGS "]
[]
[23206,"8.8.1.1",null,"Supply all labour, plant and materials and install STAINLESS STEEL LADDERS complete for chambers including stringers and rungs, chemical anchors, bolts, nuts and washers and cut to suit required length and bolted in place as per Detail on 60398/48","m",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"$f":"IF(E979 = CHAR(37), F979*G979/100,F979*G979)","v":{"v":0,"d":"0.00"}}]
[]
[23207,"8.8.1.2",null,"Supply all labour, plant and materials and install STAINLESS STEEL SAFETY CAGE for access ladder complete for chambers, cut to suit required length and bolted in place as per Dwg 60398/48","m",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E981 = CHAR(37), F981*G981/100,F981*G981)","v":{"v":0,"d":"0.00"}}]
[]
[23213,"8.8.2",null,"HANDRAILS"]
[]
[23208,"8.8.2.1",null,"Supply and install top mounted STAINLESS STEEL Handrail assembly complete with stanchions, bends and ends with chemical anchors for chamber access hatches as per Detail C on Dwg 60398/46","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E985 = CHAR(37), F985*G985/100,F985*G985)","v":{"v":0,"d":"0.00"}}]
[]
[23209,"8.8.3",null,"SUNDRY ITEMS"]
[]
[23210,null,null,"Fabricate, supply all labour, plant and materials and install the following:"]
[]
[23211,"8.8.3.1",null,"Hot Dipped Galvanised air vent as per Air Vent Detail on 60398/46","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E991 = CHAR(37), F991*G991/100,F991*G991)","v":{"v":0,"d":"0.00"}}]
[]
[23212,null,null,"Stainless pipe support steel straps/ brackets complete with neoprene etc as per Dwg 60398/16 for:"]
[]
[23215,"8.8.3.2",null,"DN100 to DN300","No.",{"v":6,"d":"6.00"},{"v":0,"d":"0.00"},{"$f":"IF(E995 = CHAR(37), F995*G995/100,F995*G995)","v":{"v":0,"d":"0.00"}}]
[]
[23219,"8.8.3.3",null,"Supply and install Type 5 valve cover (Cast into roof slab)","No.",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"$f":"IF(E997 = CHAR(37), F997*G997/100,F997*G997)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":13}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H975:H1010)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 8 - BACKWASH, SLUDGE AND BACKWASH RECOVERY SYSTEMS & "]
[null,"CHAMBERS"]
[{"$nulls":7},"SECTION 8.9: STORMWATER"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[23199,"8.9","SABS 1200LE","STORMWATER DRAINAGE"]
[]
[23200,"8.9.1","8.2.1 PSLE8.2.1","PIPES"]
[]
[23201,"8.9.1.1",null,"Supply and Install 110mm NB heavy duty solid uPVC pipes laid to fall complete with couplings, bends and tees.","m",{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"$f":"IF(E1020 = CHAR(37), F1020*G1020/100,F1020*G1020)","v":{"v":0,"d":"0.00"}}]
[]
[23202,"8.9.2","8.2.10","ACCESSORIES"]
[]
[23203,"8.9.2.1",null,"Install stormwater head wall for chambers as directed by engineer on site as per Detail 1 on DWG 60398/16","No.",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"$f":"IF(E1024 = CHAR(37), F1024*G1024/100,F1024*G1024)","v":{"v":0,"d":"0.00"}}]
[]
[23204,"8.9.2.2",null,"Construct french drain with 150mm dump rock completely wrapped in geotextile (Bidem A4 or similar approved) as directed by the Engineer. ","m³",{"v":20,"d":"20.00"},{"v":0,"d":"0.00"},{"$f":"IF(E1026 = CHAR(37), F1026*G1026/100,F1026*G1026)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":39}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H1016:H1065)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 8 - BACKWASH, SLUDGE AND BACKWASH RECOVERY SYSTEMS & "]
[null,"CHAMBERS"]
[{"$nulls":7},"SECTION 8.10: GENERAL"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[22126,"8.10",null,"GENERAL ITEMS"]
[]
[22132,"8.10.1",null,"Signage"]
[]
[22133,"8.10.1.1",null,"Supply and install signage as directed by the Engineer","Prov Sum",{"v":1,"d":"1.0"},{"v":15000,"d":"15,000.00"},{"v":15000,"d":"15,000.00"}]
[]
[22134,"8.10.1.2",null,"Overheads, charges and profit on above item 8.10.1.1","%",{"$f":"H1075","v":{"v":15000,"d":"15,000.0"}},{"v":0,"d":"0.00"},{"$f":"IF(E1077 = CHAR(37), F1077*G1077/100,F1077*G1077)","v":{"v":0,"d":"0.00"}}]
[]
[23221,"8.10.2",null,"Removal and Replacement of Backwash, Blower and Residue Disposal Pipework, Valves, Equipment and fittings"]
[]
[23222,"8.10.2.1",null,"Decommissioning and safe removal of pipework and associated fittings","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E1081 = CHAR(37), F1081*G1081/100,F1081*G1081)","v":{"v":0,"d":"0.00"}}]
[]
[23223,"8.10.2.2",null,"Supply and installation of temporary pipe supports and associated temporary support works (including scaffolding and access platforms) required to enure the safe removal of existing pipework, valves and fittings etc.","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E1083 = CHAR(37), F1083*G1083/100,F1083*G1083)","v":{"v":0,"d":"0.00"}}]
[]
[23224,"8.10.2.3",null,"Transportation of all removed pipework, valves, fittings, equipment to to EWS Depot","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E1085 = CHAR(37), F1085*G1085/100,F1085*G1085)","v":{"v":0,"d":"0.00"}}]
[]
[23225,"8.10.2.4",null,"Installation of temporary systems determined by the Contractor to ensure the continuous operation of the works. Temporary works designs are to be submitted to the Employers Agent for approval prior to proceeding with the removal of equipment","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E1087 = CHAR(37), F1087*G1087/100,F1087*G1087)","v":{"v":0,"d":"0.00"}}]
[]
[23226,"8.10.2.5",null,"Allowance for associated blank flanges and isolation valves to be utilised temporarily by the Contractor to isolate associated systems","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E1089 = CHAR(37), F1089*G1089/100,F1089*G1089)","v":{"v":0,"d":"0.00"}}]
[]
[24192,"8.10.2.6",null,"Provisional Sum for inverted U bend on blower pipework and all associated pipe supports to be determined by the Contractor, inclusive of supply, installation, miscellaneous works, pipework drawings, design and associated documentation","Prov Sum",{"v":1,"d":"1.00"},{"v":25000,"d":"25,000.00"},{"v":25000,"d":"25,000.00"}]
[]
[24193,"8.10.2.7",null,"Overheads, charges and profit on above item 8.10.1.1","%",{"$f":"H1091","v":{"v":25000,"d":"25,000.00"}},{"v":0,"d":"0.00"},{"$f":"IF(E1093 = CHAR(37), F1093*G1093/100,F1093*G1093)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":7}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H1071:H1100)","v":{"v":40000,"d":"40,000.00"}}]
[null,"SCHEDULE 8 - BACKWASH, SLUDGE AND BACKWASH RECOVERY SYSTEMS & "]
[null,"CHAMBERS"]
[{"$nulls":3},"SUMMARY OF SECTIONS"]
[null," ","SECTION","DESCRIPTION",{"$nulls":3},"AMOUNT\n(RAND)"]
[null,null,"8.1","SECTION 8.1: SITE CLEARANCE",{"$nulls":3},{"$f":"H57","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"8.2","SECTION 8.2: EARTHWORKS",{"$nulls":3},{"$f":"H108","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"8.3","SECTION 8.3: EARTHWORKS (PIPE TRENCHES)",{"$nulls":3},{"$f":"H157","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"8.4","SECTION 8.4: CONCRETE (STRUCTURAL)",{"$nulls":3},{"$f":"H331","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"8.5","SECTION 8.5: MEDIUM PRESSURE PIPELINES (STEEL)",{"$nulls":3},{"$f":"H512","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"8.6","SECTION 8.6: PIPEWORK ASSEMBLIES",{"$nulls":3},{"$f":"H915","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"8.7","SECTION 8.7: BEDDING",{"$nulls":3},{"$f":"H970","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"8.8","SECTION 8.8: STRUCTURAL STEELWORK (SUNDRY ITEMS) AND GRP",{"$nulls":3},{"$f":"H1011","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"8.9","SECTION 8.9: STORMWATER",{"$nulls":3},{"$f":"H1066","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"8.10","SECTION 8.10: GENERAL",{"$nulls":3},{"$f":"H1101","v":{"v":40000,"d":"40,000.00"}}]
{"$rows_empty":39}
[null,null," Total Carried Forward To Summary Of Schedules"," Total Carried Forward To Summary Of Schedules",{"$nulls":3},{"$f":"SUM(H1106:H1163)","v":{"v":40000,"d":"40,000.00"}}]

{"sheet":"Schedule 9","index":8,"n_rows":212,"n_cols":8,"rows_kept":212}
["Rate=G","SCHEDULE 9 - CLARIFIERS"]
[{"$nulls":7},"SECTION 9.1: STRUCTURAL STEELWORK"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[22358,"9.1","SANS 1200 H, PSAHA, PACP","STRUCTURAL STEELWORK"]
[]
[22359,"9.1.1","PSHA 8.3","SUPPLY AND FABRICATION"]
[]
[22360,"9.1.1.1","8.3.1.1","Preparation of shop detail drawings","t",12.3,{"v":0,"d":"0.00"},{"$f":"IF(E8 = CHAR(37), F8*G8/100,F8*G8)","v":{"v":0,"d":"0.00"}}]
[]
[22379,null,"8.3.1.2","Supply and fabrication of steelwork in S355JR steel complete with all necessary cleats, brackets, gussets, base plates, packs, grade 8.8 bolts, holes, welding, shaping, etc."]
[]
[22387,"9.1.1.2",null,"Beams over clarifiers","t",0.4,{"v":0,"d":"0.00"},{"$f":"IF(E12 = CHAR(37), F12*G12/100,F12*G12)","v":{"v":0,"d":"0.00"}}]
[]
[22381,"9.1.1.3",null,"Walkway over clarifiers","t",2.4,{"v":0,"d":"0.00"},{"$f":"IF(E14 = CHAR(37), F14*G14/100,F14*G14)","v":{"v":0,"d":"0.00"}}]
[]
[22361,"9.1.2","PSHA 8.3","DELIVERY"]
[]
[22362,"9.1.2.1","8.3.2.1","Normal load","t",{"v":3,"d":"3.0"},{"v":0,"d":"0.00"},{"$f":"IF(E18 = CHAR(37), F18*G18/100,F18*G18)","v":{"v":0,"d":"0.00"}}]
[]
[22363,"9.1.3","PSHA 8.3","ERECTION"]
[]
[22364,"9.1.3.1","8.3.3","Offloading, stacking on site, and erection of steelwork","t",{"v":3,"d":"3.0"},{"v":0,"d":"0.00"},{"$f":"IF(E22 = CHAR(37), F22*G22/100,F22*G22)","v":{"v":0,"d":"0.00"}}]
[]
[22365,"9.1.4","PSHA 8.3","SITE WELDING"]
[]
[22366,"9.1.4.1","8.3.5","Site weld walkway items as appropriate","m",{"v":60,"d":"60.0"},{"v":0,"d":"0.00"},{"$f":"IF(E26 = CHAR(37), F26*G26/100,F26*G26)","v":{"v":0,"d":"0.00"}}]
[]
[22367,"9.1.5","PSHA 8.3","HANDRAILS"]
[]
[22368,null,"8.3.7 b)","Supply, apply corrosion protection, paint, and install steel handrail assembly complete with stanchions, bends and ends with chemical anchors to detail on dwg 60398/12"]
[]
[22369,"9.1.5.1","8.3.7 b) 1)","Horizontal (hand and knee rails)","m",{"v":200,"d":"200.0"},{"v":0,"d":"0.00"},{"$f":"IF(E32 = CHAR(37), F32*G32/100,F32*G32)","v":{"v":0,"d":"0.00"}}]
[]
[22370,"9.1.5.2","8.3.7 b) 2)","Sloping","m",{"v":50,"d":"50.0"},{"v":0,"d":"0.00"},{"$f":"IF(E34 = CHAR(37), F34*G34/100,F34*G34)","v":{"v":0,"d":"0.00"}}]
[]
[22371,"9.1.5.3","8.3.7 b) 3)","Shaped ends and bends","No.",{"v":40,"d":"40.0"},{"v":0,"d":"0.00"},{"$f":"IF(E36 = CHAR(37), F36*G36/100,F36*G36)","v":{"v":0,"d":"0.00"}}]
[]
[22391,"9.1.5.4",null,"Allow for a life saving floatation device to be mounted on handrailing. To include mounting and life saving device","No.",{"v":3,"d":"3.0"},{"v":0,"d":"0.00"},{"$f":"IF(E38 = CHAR(37), F38*G38/100,F38*G38)","v":{"v":0,"d":"0.00"}}]
[]
[22376,"9.1.6","PSHA 8.3","WALKWAYS"]
[]
[22355,null,"8.3.9","Open grid floors in S355JR steel including access hatch as indicated on drawing 60398/12"]
[]
[]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H4:H45)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 9 - CLARIFIERS"]
[{"$nulls":7},"SECTION 9.1: STRUCTURAL STEELWORK"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H46","v":{"v":0,"d":"0.00"}}]
[22390,"9.1.6.1",null,"Design, prepare shop detail drawings, supply all materials, apply corrosion protection, and install, open grated walkway and steps complete over clarifiers and fixed to concrete with anchors","Sum",{"v":1,"d":"1.0"},{"v":0,"d":"0.00"},{"$f":"IF(E51 = CHAR(37), F51*G51/100,F51*G51)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":52}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H50:H103)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 9 - CLARIFIERS"]
[{"$nulls":7},"SECTION 9.2: OTHER"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[20420,"9.2",null,"OTHER"]
[]
[20421,"9.2.1",null,"Provisional sum for the design, supply, associated ancillary works and installation of new pipework within Clarifiers, including associated supports and brackets achored to clarifier walls.","Prov Sum",{"v":1,"d":"1.00"},{"v":250000,"d":"250,000.00"},{"v":250000,"d":"250,000.00"}]
[]
[23809,"9.2.2",null,"Overheads & profit on above item","%",{"$f":"H110","v":{"v":250000,"d":"250,000.00"}},{"v":0,"d":"0.00"},{"$f":"IF(E112 = CHAR(37), F112*G112/100,F112*G112)","v":{"v":0,"d":"0.00"}}]
[]
[23297,"9.2.3",null,"Provisional sum for the design, supply, associated ancillary works and installation of brickwork within main inlet channel, including associated achorage to channel walls.","Prov Sum",{"v":1,"d":"1.00"},{"v":10000,"d":"10,000.00"},{"v":10000,"d":"10,000.00"}]
[]
[23810,"9.2.4",null,"Overheads & profit on above item","%",{"$f":"H114","v":{"v":10000,"d":"10,000.00"}},{"v":0,"d":"0.00"},{"$f":"IF(E116 = CHAR(37), F116*G116/100,F116*G116)","v":{"v":0,"d":"0.00"}}]
[]
[24175,"9.2.5",null,"Provisional sum for the design, supply, associated ancillary works and installation of an overflow from the clear wate reservoir to the backwash recovery tank.","Prov Sum",{"v":1,"d":"1.00"},{"v":75000,"d":"75,000.00"},{"v":75000,"d":"75,000.00"}]
[]
[24176,"9.2.6",null,"Overheads & profit on above item","%",{"$f":"H118","v":{"v":75000,"d":"75,000.00"}},{"v":0,"d":"0.00"},{"$f":"IF(E120 = CHAR(37), F120*G120/100,F120*G120)","v":{"v":0,"d":"0.00"}}]
[]
[24184,"9.2.7","SANS1200H\r\nPSH","Design, supply and install steel walkway above raw water channel between clarifiers inclusive of associated supports, frame, coating and ancillary works \r\n","m²",{"v":45,"d":"45.00"},{"v":0,"d":"0.00"},{"$f":"IF(E122 = CHAR(37), F122*G122/100,F122*G122)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":27}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H108:H149)","v":{"v":335000,"d":"335,000.00"}}]
[null,"SCHEDULE 9 - CLARIFIERS"]
[{"$nulls":3},"SUMMARY OF SECTIONS"]
[null," ","SECTION","DESCRIPTION",{"$nulls":3},"AMOUNT\n(RAND)"]
[null,null,"9.1","SECTION 9.1: STRUCTURAL STEELWORK",{"$nulls":3},{"$f":"H104","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"9.2","SECTION 9.2: OTHER",{"$nulls":3},{"$f":"H150","v":{"v":335000,"d":"335,000.00"}}]
{"$rows_empty":55}
[null,null," Total Carried Forward To Summary Of Schedules"," Total Carried Forward To Summary Of Schedules",{"$nulls":3},{"$f":"SUM(H154:H211)","v":{"v":335000,"d":"335,000.00"}}]

{"sheet":"Schedule 10","index":9,"n_rows":224,"n_cols":8,"rows_kept":224}
["Rate=G","SCHEDULE 10 - BACKWASH RECOVERY TANK"]
[{"$nulls":7},"SECTION 10.1: STRUCTURAL STEELWORK (SUNDRY ITEMS) AND GRP"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[23802,"10.1","SABS 1200 H","STRUCTURAL STEELWORK (SUNDRY ITEMS) AND GRP"]
[]
[23803,"10.1.1",null,"SUNDRY ITEMS"]
[]
[23804,"10.1.1.1",null,"Supply and install steel staircase next to tank 1000mm high","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E8 = CHAR(37), F8*G8/100,F8*G8)","v":{"v":0,"d":"0.00"}}]
[]
[23808,"10.1.1.2",null,"Design, supply and install steel walkway above backwash recovery tank inclusive of associated supports, frame, coating and ancillary works (3300mm x 21600mm)\r\n","m²",{"v":80,"d":"80.00"},{"v":0,"d":"0.00"},{"$f":"IF(E10 = CHAR(37), F10*G10/100,F10*G10)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":46}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H4:H56)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 10 - BACKWASH RECOVERY TANK"]
[{"$nulls":7},"SECTION 10.2: OTHER"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[23261,"10.2",null,"OTHER"]
[]
[23262,"10.2.1",null,"Provisional sum for increase in overflow from backwash recovery tank","Prov Sum",{"v":1,"d":"1.00"},{"v":15000,"d":"15,000.00"},{"v":15000,"d":"15,000.00"}]
[]
[23800,"10.2.2",null,"Overheads and Profit on the above item","%",{"$f":"H63","v":{"v":15000,"d":"15,000.00"}},{"v":0,"d":"0.00"},{"$f":"IF(E65 = CHAR(37), F65*G65/100,F65*G65)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":53}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H61:H118)","v":{"v":15000,"d":"15,000.00"}}]
[null,"SCHEDULE 10 - BACKWASH RECOVERY TANK"]
[{"$nulls":7},"SECTION 10.3: PIPEWORK ASSEMBLIES"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[23342,"10.3","SANS 1200 L, PSL","PIPEWORK ASSEMBLIES"]
[]
[23324,null,null,"Fabricate, supply and install valves, spool pieces, fittings and bends complete inclusive of all collar/ crotch plate reinforcing with internal and external coating as per specifications. Rates to include for all bolts, nuts, gaskets and jointing material, testing, holiday detection, radiographic inspection of field welds, preparation for welding where required and the repair and making good of all linings and coatings. "]
[]
[23359,"10.3.1","8.2.5\r\nPSL 8.2.5","DN100 DRAINAGE PIPEWORK FROM FILTER PLENUM"]
[]
[23355,null,null,"All flanges to be supplied and as per SANS 1123 Table 1600/3 unless otherwise shown or specified "]
[]
[23343,"10.3.1.1",null,"DN100 Wedge Gate Valve PN16 with hand wheel and extended spindle","No.",{"v":6,"d":"6.0"},{"v":0,"d":"0.00"},{"$f":"IF(E131 = CHAR(37), F131*G131/100,F131*G131)","v":{"v":0,"d":"0.00"}}]
[]
[23344,"10.3.1.2",null,"DN100 90 degree (ANSI) B16.9 long radius bend with 300mm long spool piece welded to one end and other end flanged, flange to match valve (Final Lengths to be determined on site) ","No.",{"v":6,"d":"6.0"},{"v":0,"d":"0.00"},{"$f":"IF(E133 = CHAR(37), F133*G133/100,F133*G133)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":28}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H123:H161)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 10 - BACKWASH RECOVERY TANK"]
[{"$nulls":3},"SUMMARY OF SECTIONS"]
[null," ","SECTION","DESCRIPTION",{"$nulls":3},"AMOUNT\n(RAND)"]
[null,null,"10.1","SECTION 10.1: STRUCTURAL STEELWORK (SUNDRY ITEMS) AND GRP",{"$nulls":3},{"$f":"H57","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"10.2","SECTION 10.2: OTHER",{"$nulls":3},{"$f":"H119","v":{"v":15000,"d":"15,000.00"}}]
[]
[null,null,"10.3","SECTION 10.3: PIPEWORK ASSEMBLIES",{"$nulls":3},{"$f":"H162","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":53}
[null,null," Total Carried Forward To Summary Of Schedules"," Total Carried Forward To Summary Of Schedules",{"$nulls":3},{"$f":"SUM(H166:H223)","v":{"v":15000,"d":"15,000.00"}}]

{"sheet":"Schedule 11","index":10,"n_rows":293,"n_cols":8,"rows_kept":293}
["Rate=G","SCHEDULE 11 - ROADS"]
[{"$nulls":7},"SECTION 11.1: EARTHWORKS (ROADS, SUBGRADE)"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[18620,"11.1","SABS 1200 DM","EARTHWORKS"]
[]
[18621,"11.1.1",null,"ROAD-BED PREPARATION"]
[]
[18622,null,"8.3.3 (a)","Road-bed preparation and compaction of material to:"]
[]
[18623,"11.1.1.1","8.3.3 (a) (1)","Compact to 93% MOD AASHTO maximum density","m³",{"v":100,"d":"100.00"},{"v":0,"d":"0.00"},{"$f":"IF(E10 = CHAR(37), F10*G10/100,F10*G10)","v":{"v":0,"d":"0.00"}}]
[]
[18625,"11.1.2",null,"EARTHWORKS"]
[]
[20834,null,"8.3.4","Cut to fill"]
[]
[20835,"11.1.2.1",null,"Compact to 93% MOD AASHTO maximum density","m³",{"v":110,"d":"110.00"},{"v":0,"d":"0.00"},{"$f":"IF(E16 = CHAR(37), F16*G16/100,F16*G16)","v":{"v":0,"d":"0.00"}}]
[]
[20836,null,"8.3.4","Borrow to fill"]
[]
[20837,"11.1.2.2",null,"Compact to 93% MOD AASHTO maximum density","m³",{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"$f":"IF(E20 = CHAR(37), F20*G20/100,F20*G20)","v":{"v":0,"d":"0.00"}}]
[]
[18616,null,"8.3.7","Cut to spoil (Provisional):"]
[]
[18617,"11.1.2.3","8.3.7(a)","a) Soft excavation","m³",{"v":160,"d":"160.00"},{"v":0,"d":"0.00"},{"$f":"IF(E24 = CHAR(37), F24*G24/100,F24*G24)","v":{"v":0,"d":"0.00"}}]
[]
[18618,"11.1.2.4","8.3.7(b)","b) Intermediate excavation","m³",{"v":150,"d":"150.00"},{"v":0,"d":"0.00"},{"$f":"IF(E26 = CHAR(37), F26*G26/100,F26*G26)","v":{"v":0,"d":"0.00"}}]
[]
[18619,"11.1.2.5","8.3.7(c)","c) Hard excavation","m³",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E28 = CHAR(37), F28*G28/100,F28*G28)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":31}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H4:H59)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 11 - ROADS"]
[{"$nulls":7},"SECTION 11.2: ROAD REINSTATEMENT"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[18635,"11.2",null,"ACCESS ROAD REINSTATEMENT"]
[]
[18615,"11.2.1","SABS 1200 ME\r\nPSME","SELECTED LAYER/SUBBASE"]
[]
[18624,"11.2.1.1",null,"Construct 200mm thick G7 subbase course with material from commercial sources and compact to 95% MOD AASHTO","m³",{"v":130,"d":"130.00"},{"v":0,"d":"0.00"},{"$f":"IF(E68 = CHAR(37), F68*G68/100,F68*G68)","v":{"v":0,"d":"0.00"}}]
[]
[18636,"11.2.2","SABS 1200 MF\r\nPSMF","BASE/ WEARING COURSE"]
[]
[18637,"11.2.2.1","8.3.3","Construct 100mm thick G2 base course with material from commercial sources and compact to 98% MOD AASHTO","m³",{"v":70,"d":"70.00"},{"v":0,"d":"0.00"},{"$f":"IF(E72 = CHAR(37), F72*G72/100,F72*G72)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":43}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H64:H115)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 11 - ROADS"]
[{"$nulls":7},"SECTION 11.3: SURFACING "]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[18638,"11.3","SANS 1200MH","SURFACING "]
[]
[18639,"11.3.1","SANS 1200 MH\r\nPSMH","ASPHALT SURFACING"]
[]
[18640,null,null,"Continuously medium graded asphalt surfacing using 35/50 Pen. Grade bitumen: "]
[]
[18641,"11.3.1.1","PSMH 8.5.4","40mm to roads","m²",{"v":650,"d":"650.00"},{"v":0,"d":"0.00"},{"$f":"IF(E126 = CHAR(37), F126*G126/100,F126*G126)","v":{"v":0,"d":"0.00"}}]
[]
[20887,"11.3.1.2","8.5.1","Prime Coat (MC30 cutback bitumen)","m²",{"v":650,"d":"650.00"},{"v":0,"d":"0.00"},{"$f":"IF(E128 = CHAR(37), F128*G128/100,F128*G128)","v":{"v":0,"d":"0.00"}}]
[]
[20888,"11.3.1.3","8.5.3\r\nPSMH 3.3","Tack coat","m²",{"v":650,"d":"650.00"},{"v":0,"d":"0.00"},{"$f":"IF(E130 = CHAR(37), F130*G130/100,F130*G130)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":45}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H120:H175)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 11 - ROADS"]
[{"$nulls":7},"SECTION 11.4: CONCRETE KERBING AND CHANNELLING "]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[18627,"11.4","SANS 1200 MK","CONCRETE KERBING AND CHANNELLING "]
[]
[18626,"11.4.1",null,"KERBING"]
[]
[18628,null,"8.2.1","Fig 6 barrier kerb and cast insitu 25Mpa filler/ channel complete as per detail with continuous 120 x 100mm haunch, for:"]
[]
[18629,"11.4.1.1",null,"Straight kerbing and radii in excess of 20m","m",{"v":260,"d":"260.00"},{"v":0,"d":"0.00"},{"$f":"IF(E186 = CHAR(37), F186*G186/100,F186*G186)","v":{"v":0,"d":"0.00"}}]
[]
[18630,"11.4.1.2",null,"Radii that are greater than 4.0m - 20m in radius","m",{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"$f":"IF(E188 = CHAR(37), F188*G188/100,F188*G188)","v":{"v":0,"d":"0.00"}}]
[]
[18631,"11.4.1.3",null,"Radii that are greater than 1.0m - 4.0m in radius (Provisional Quantity) ","m",{"v":25,"d":"25.00"},{"v":0,"d":"0.00"},{"$f":"IF(E190 = CHAR(37), F190*G190/100,F190*G190)","v":{"v":0,"d":"0.00"}}]
[]
[18632,"11.4.2","8.2.6","ANCILLARIES "]
[]
[18633,null,null,"Cast in-situ transitions: "]
[]
[18634,"11.4.2.1","8.2.6.2","Concrete, specified strength 25MPa complete with formwork and reinforcing mesh","m³",{"v":20,"d":"20.00"},{"v":0,"d":"0.00"},{"$f":"IF(E196 = CHAR(37), F196*G196/100,F196*G196)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":34}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H180:H230)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 11 - ROADS"]
[{"$nulls":3},"SUMMARY OF SECTIONS"]
[null," ","SECTION","DESCRIPTION",{"$nulls":3},"AMOUNT\n(RAND)"]
[null,null,"11.1","SECTION 11.1: EARTHWORKS (ROADS, SUBGRADE)",{"$nulls":3},{"$f":"H60","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"11.2","SECTION 11.2: ROAD REINSTATEMENT",{"$nulls":3},{"$f":"H116","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"11.3","SECTION 11.3: SURFACING ",{"$nulls":3},{"$f":"H176","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"11.4","SECTION 11.4: CONCRETE KERBING AND CHANNELLING ",{"$nulls":3},{"$f":"H231","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":51}
[null,null," Total Carried Forward To Summary Of Schedules"," Total Carried Forward To Summary Of Schedules",{"$nulls":3},{"$f":"SUM(H235:H292)","v":{"v":0,"d":"0.00"}}]

{"sheet":"Schedule 12","index":11,"n_rows":202,"n_cols":8,"rows_kept":202}
["Rate=G","SCHEDULE 12 - STORMWATER"]
[{"$nulls":7},"SECTION 12.1: STORMWATER"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[18892,"12.1","SABS 1200LE","STORMWATER DRAINAGE"]
[]
[18893,"12.1.1",null,"PIPES"]
[]
[18897,null,null,"Supply and lay stormwater drainage pipes for the following:"]
[]
[18894,"12.1.1.1","PSLE 8.2.1","Supply and Install up to 110mm NB heavy duty solid uPVC pipes laid to fall complete with couplings, bends and tees.","m",{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"$f":"IF(E10 = CHAR(37), F10*G10/100,F10*G10)","v":{"v":0,"d":"0.00"}}]
[]
[18898,"12.1.1.2","PSLE 8.2.1\r\n","Supply and Install 160mm NB heavy duty solid uPVC pipes laid to fall complete with couplings, bends and tees.","m",{"v":30,"d":"30.00"},{"v":0,"d":"0.00"},{"$f":"IF(E12 = CHAR(37), F12*G12/100,F12*G12)","v":{"v":0,"d":"0.00"}}]
[]
[18899,"12.1.1.3","PSLE 8.2.1\r\n","Supply and Install 200 to 350mm NB heavy duty solid uPVC pipes laid to fall complete with couplings, bends and tees.","m",{"v":30,"d":"30.00"},{"v":0,"d":"0.00"},{"$f":"IF(E14 = CHAR(37), F14*G14/100,F14*G14)","v":{"v":0,"d":"0.00"}}]
[]
[18895,"12.1.2",null,"ACCESSORIES"]
[]
[18896,"12.1.2.1","PSLE 8.2.15","Install stormwater chambers inclusive of grating or MH cover as directed by engineer on site as per Dwg 60398/46","No.",{"v":8,"d":"8.00"},{"v":0,"d":"0.00"},{"$f":"IF(E18 = CHAR(37), F18*G18/100,F18*G18)","v":{"v":0,"d":"0.00"}}]
[]
[18901,"12.1.2.2","PSLE 8.2.16","Install stormwater head wall for stormwater outlets as directed by engineer on site as per Dwg 60398/46(All sizes)","No.",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"$f":"IF(E20 = CHAR(37), F20*G20/100,F20*G20)","v":{"v":0,"d":"0.00"}}]
[]
[20864,"12.1.2.3",null,"Supply and construct 570mm wide Kalvis Type 01 water channel inclusive of all jointing and ground preparation for straight sections. Rate inclusive of grating.\r\n","m",{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"$f":"IF(E22 = CHAR(37), F22*G22/100,F22*G22)","v":{"v":0,"d":"0.00"}}]
[]
[23508,"12.1.2.4",null,"Supply and construct 650mm wide Kalvis Type 02 water channel inclusive of all jointing and ground preparation for straight sections.","m",{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"$f":"IF(E24 = CHAR(37), F24*G24/100,F24*G24)","v":{"v":0,"d":"0.00"}}]
[]
[23509,"12.1.2.5",null,"Supply and construct 1000mm x 570mm x 300mm Kalvis Type 01 water channel inclusive of all jointing and ground preparation for straight sections and inclusive of GMS grating.","m",{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"$f":"IF(E26 = CHAR(37), F26*G26/100,F26*G26)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":10}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H4:H36)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 12 - STORMWATER"]
[{"$nulls":7},"SECTION 12.2: EARTHWORKS (PIPE TRENCHES)"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[20838,"12.2","SABS1200 DB","EARTHWORKS (PIPE TRENCHES)"]
[]
[20839,"12.2.1","PSDB 5.2 8.3.2","EXCAVATION"]
[]
[20844,null,"8.3.2 (a) PSDB 8.3.2 (a)","Excavate in all materials for pipe trenches, backfill, compact to specification and dispose of surplus/unsuitable material, for pipes:"]
[]
[20845,null,null,"Up to DN350 pipeline for a total trench depth"]
[]
[20846,"12.2.1.1",null,"Up to 3.0m","m³",{"v":150,"d":"150.00"},{"v":0,"d":"0.00"},{"$f":"IF(E49 = CHAR(37), F49*G49/100,F49*G49)","v":{"v":0,"d":"0.00"}}]
[]
[20847,null,"8.3.2 (b) PSDB 8.3.2 (b)","Extra-over Item 12.2.1.1 for excavation in (All provisional):"]
[]
[20848,"12.2.1.2",null,"1) Intermediate excavation","m³",{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"$f":"IF(E53 = CHAR(37), F53*G53/100,F53*G53)","v":{"v":0,"d":"0.00"}}]
[]
[20849,"12.2.1.3",null,"2) Hard rock excavation","m³",{"v":20,"d":"20.00"},{"v":0,"d":"0.00"},{"$f":"IF(E55 = CHAR(37), F55*G55/100,F55*G55)","v":{"v":0,"d":"0.00"}}]
[]
[20850,"12.2.1.4",null,"3) Boulder Excavation class A (Provisional)","m³",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E57 = CHAR(37), F57*G57/100,F57*G57)","v":{"v":0,"d":"0.00"}}]
[]
[20851,"12.2.1.5",null,"4) Boulder Excavation class B (Provisional)","m³",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E59 = CHAR(37), F59*G59/100,F59*G59)","v":{"v":0,"d":"0.00"}}]
[]
[20852,"12.2.1.6",null,"Hand excavation and backfill where ordered by the Engineer (Provisional Quantity)","m³",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E61 = CHAR(37), F61*G61/100,F61*G61)","v":{"v":0,"d":"0.00"}}]
[]
[20853,"12.2.1.7","8.3.2 (c)","Excavate and dispose of unsuitable material from trench bottom (Provisional)","m³",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E63 = CHAR(37), F63*G63/100,F63*G63)","v":{"v":0,"d":"0.00"}}]
[]
[20854,"12.2.1.8",null,"Hand excavation to prove existing services (Provisional)","m³",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E65 = CHAR(37), F65*G65/100,F65*G65)","v":{"v":0,"d":"0.00"}}]
[]
[20840,"12.2.2","8.3.3","EXCAVATION ANCILLARIES "]
[]
[20841,null,null,"Make up deficiency in backfill material (Provisional)"]
[]
[20842,"12.2.2.1","8.3.3.1 (a)","a) from other necessary excavations on site","m³",{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"$f":"IF(E71 = CHAR(37), F71*G71/100,F71*G71)","v":{"v":0,"d":"0.00"}}]
[]
[20843,"12.2.2.2","8.3.3.1 (c)","b) by importation from commercial sources","m³",{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"$f":"IF(E73 = CHAR(37), F73*G73/100,F73*G73)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":12}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H41:H85)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 12 - STORMWATER"]
[{"$nulls":7},"SECTION 12.3: BEDDING"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[20855,"12.3","SABS 1200 LB","BEDDING (PIPES)"]
[]
[20863,"12.3.1","PSLB 8.2.1","Provision of bedding from trench excavations:"]
[]
[20856,"12.3.1.1",null,"Selected granular material for 200mm bedding cradle below pipe invert","m³",{"v":15,"d":"15.00"},{"v":0,"d":"0.00"},{"$f":"IF(E94 = CHAR(37), F94*G94/100,F94*G94)","v":{"v":0,"d":"0.00"}}]
[]
[20857,"12.3.1.2",null,"Selected granular material for fill blanket to 300mm above pipe crown","m³",{"v":25,"d":"25.00"},{"v":0,"d":"0.00"},{"$f":"IF(E96 = CHAR(37), F96*G96/100,F96*G96)","v":{"v":0,"d":"0.00"}}]
[]
[20859,"12.3.1.3","PSLB 8.2.1.1","Extra Over for screening of material from the trench excavation, to achieve grading suitable to comply with the bedding and blanket material specification (Provisional Quantity) ","m³",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E98 = CHAR(37), F98*G98/100,F98*G98)","v":{"v":0,"d":"0.00"}}]
[]
[20860,"12.3.2","PSLB 8.2.2","Supply only of bedding by importation:"]
[]
[20861,null,"PSLB 8.2.2.3","From commercial sources:"]
[]
[20862,"12.3.2.1",null,"a) Selected granular material for 200mm bedding cradle below pipe invert","m³",{"v":15,"d":"15.00"},{"v":0,"d":"0.00"},{"$f":"IF(E104 = CHAR(37), F104*G104/100,F104*G104)","v":{"v":0,"d":"0.00"}}]
[]
[20858,"12.3.2.2",null,"b) Selected granular material for fill blanket to 300mm above pipe crown","m³",{"v":25,"d":"25.00"},{"v":0,"d":"0.00"},{"$f":"IF(E106 = CHAR(37), F106*G106/100,F106*G106)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":33}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H90:H139)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 12 - STORMWATER"]
[{"$nulls":3},"SUMMARY OF SECTIONS"]
[null," ","SECTION","DESCRIPTION",{"$nulls":3},"AMOUNT\n(RAND)"]
[null,null,"12.1","SECTION 12.1: STORMWATER",{"$nulls":3},{"$f":"H37","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"12.2","SECTION 12.2: EARTHWORKS (PIPE TRENCHES)",{"$nulls":3},{"$f":"H86","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"12.3","SECTION 12.3: BEDDING",{"$nulls":3},{"$f":"H140","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":53}
[null,null," Total Carried Forward To Summary Of Schedules"," Total Carried Forward To Summary Of Schedules",{"$nulls":3},{"$f":"SUM(H144:H201)","v":{"v":0,"d":"0.00"}}]

{"sheet":"Schedule 13","index":12,"n_rows":332,"n_cols":8,"rows_kept":332}
["Rate=G","SCHEDULE 13 - MISCELLANEOUS WORKS"]
[{"$nulls":7},"SECTION 13.1: SITE CLEARANCE"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[16907,"13.1","SANS 1200 C, PSC","SITE CLEARANCE"]
[]
[16762,"13.1.1",null,"CLEAR SITE"]
[]
[16908,null,"8.2.1","Clear and grub:"]
[]
[16909,"13.1.1.1",null,"Water Treatment Works site","m²",{"v":500,"d":"500.00"},{"v":0,"d":"0.00"},{"$f":"IF(E10 = CHAR(37), F10*G10/100,F10*G10)","v":{"v":0,"d":"0.00"}}]
[]
[16910,null,"8.2.4\r\nPSC 8.2.4","Re-clear surfaces where directed by Engineer (Provisional):"]
[]
[16911,"13.1.1.2",null,"Water Treatment Works site","m²",{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"$f":"IF(E14 = CHAR(37), F14*G14/100,F14*G14)","v":{"v":0,"d":"0.00"}}]
[]
[16763,"13.1.2",null,"REMOVE TOPSOIL AND OTHER SURFACES"]
[]
[16760,null,"8.2.10 PSC 8.2.10","Remove topsoil, stockpile, maintain and dispose of surplus to nominal depth of 150mm, for:"]
[]
[16761,"13.1.2.1",null,"Fill embankments and designated areas","m³",{"v":20,"d":"20.00"},{"v":0,"d":"0.00"},{"$f":"IF(E20 = CHAR(37), F20*G20/100,F20*G20)","v":{"v":0,"d":"0.00"}}]
[]
[16645,null,"PSC 8.2.11","Saw cutting of existing asphalt of thickness: "]
[]
[16913,"13.1.2.2",null,"30 - 60mm","m",{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"$f":"IF(E24 = CHAR(37), F24*G24/100,F24*G24)","v":{"v":0,"d":"0.00"}}]
[]
[16914,"13.1.2.3","PSC 8.2.13","Remove existing road asphalt surfacing and spoil at approved disposal sites (25 to 45mm thickness) ","m²",{"v":150,"d":"150.00"},{"v":0,"d":"0.00"},{"$f":"IF(E26 = CHAR(37), F26*G26/100,F26*G26)","v":{"v":0,"d":"0.00"}}]
[]
[16915,null,"PSC 8.2.14","Remove existing gravel layer works to spoil"]
[]
[16916,"13.1.2.4",null,"Gravel and crushed stone layer works  to roads           ","m³",{"v":30,"d":"30.00"},{"v":0,"d":"0.00"},{"$f":"IF(E30 = CHAR(37), F30*G30/100,F30*G30)","v":{"v":0,"d":"0.00"}}]
[]
[16755,null,"PSC 8.2.18","Remove along edges of road, driveways and footway channel (provisional quantity): "]
[]
[16754,"13.1.2.5",null,"a) All pre-cast concrete kerbing and channelling","m",{"v":20,"d":"20.00"},{"v":0,"d":"0.00"},{"$f":"IF(E34 = CHAR(37), F34*G34/100,F34*G34)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":15}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H4:H49)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 13 - MISCELLANEOUS WORKS"]
[{"$nulls":7},"SECTION 13.2: GABIONS AND PITCHING"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[16943,"13.2","SANS 1200 DK","GABIONS AND PITCHING"]
[]
[16944,"13.2.1","8.2.1","SURFACE PREPARATION"]
[]
[16945,null,null,"Surface preparation for bedding:"]
[]
[16890,"13.2.1.1","8.2.1(a)","Cavities filled with approved excavated material or rock (Provisional Quantity)","m²",{"v":15,"d":"15.00"},{"v":0,"d":"0.00"},{"$f":"IF(E60 = CHAR(37), F60*G60/100,F60*G60)","v":{"v":0,"d":"0.00"}}]
[]
[16717,"13.2.1.2","8.2.1(b)","Cavities filled with 15MPa concrete ","m²",{"v":15,"d":"15.00"},{"v":0,"d":"0.00"},{"$f":"IF(E62 = CHAR(37), F62*G62/100,F62*G62)","v":{"v":0,"d":"0.00"}}]
[]
[16718,"13.2.2","PSDK 8.2.8","EXCAVATION"]
[]
[16719,null,null,"Excavate in all materials, backfill, compact, and dispose of surplus/unsuitable material:"]
[]
[16651,"13.2.2.1",null,"For gabions and reno mattress baskets","m³",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E68 = CHAR(37), F68*G68/100,F68*G68)","v":{"v":0,"d":"0.00"}}]
[]
[16652,"13.2.3","PSDK 3.1.2","GABIONS"]
[]
[16653,null,"8.2.2 PSDK 8.2.2","Supply and Construct gabions complete with hand rock using double twisted hexagonal mesh type 80 with 3.4mm OD frame wire and 2.7mm OD mesh wire to SANS 1580:2005 coated in Galfan (provisional quantities), for:"]
[]
[16654,"13.2.3.1",null,"Reno Mattresses of depth 0,3 m with diaphragms providing 2,0 m x 1,0 m cells ","m³",{"v":6,"d":"6.00"},{"v":0,"d":"0.00"},{"$f":"IF(E74 = CHAR(37), F74*G74/100,F74*G74)","v":{"v":0,"d":"0.00"}}]
[]
[16709,"13.2.3.2",null,"Gabions of section 2,0 m x 1,0 m x 0,5m high","m³",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E76 = CHAR(37), F76*G76/100,F76*G76)","v":{"v":0,"d":"0.00"}}]
[]
[16634,"13.2.3.3",null,"Gabions of section 2,0 m x 1,0 m x 1,0m high","m³",{"v":30,"d":"30.00"},{"v":0,"d":"0.00"},{"$f":"IF(E78 = CHAR(37), F78*G78/100,F78*G78)","v":{"v":0,"d":"0.00"}}]
[]
[16635,"13.2.4","8.2.4, PSDK 8.2.4","GEOTEXTILE (GRADE A4)"]
[]
[16636,"13.2.4.1",null,"Supply and install below gabions and reno mattress baskets","m²",{"v":15,"d":"15.00"},{"v":0,"d":"0.00"},{"$f":"IF(E82 = CHAR(37), F82*G82/100,F82*G82)","v":{"v":0,"d":"0.00"}}]
[]
[16637,"13.2.5","8.2.5","STONE PITCHING"]
[]
[16638,"13.2.5.1",null,"Stone pitching with 150mm dump rock, grouted, where directed by the Engineer","m³",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E86 = CHAR(37), F86*G86/100,F86*G86)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":10}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H54:H96)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 13 - MISCELLANEOUS WORKS"]
[{"$nulls":7},"SECTION 13.3: CONCRETE (STRUCTURAL)"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[16639,"13.3","SABS 1200 G","CONCRETE (STRUCTURAL)"]
[]
[18732,"13.3.1",null,"MISCELLANEOUS"]
[]
[18733,null,null,"Concrete retaining block walling inclusive of concrete base 15Mpa, subsoil drain and geotextile :"]
[]
[18734,"13.3.1.1",null,"a) Terraforce Blok or similar approved - Retaining Blocks L300","m²",{"v":20,"d":"20.00"},{"v":0,"d":"0.00"},{"$f":"IF(E107 = CHAR(37), F107*G107/100,F107*G107)","v":{"v":0,"d":"0.00"}}]
[]
[18735,"13.3.1.2",null,"b) Loffelstein or similar approved L500 blocks","m²",{"v":20,"d":"20.00"},{"v":0,"d":"0.00"},{"$f":"IF(E109 = CHAR(37), F109*G109/100,F109*G109)","v":{"v":0,"d":"0.00"}}]
[]
[18736,"13.3.1.3",null,"c) Loffelstein or similar approved L750 blocks","m²",{"v":20,"d":"20.00"},{"v":0,"d":"0.00"},{"$f":"IF(E111 = CHAR(37), F111*G111/100,F111*G111)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":44}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H101:H155)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 13 - MISCELLANEOUS WORKS"]
[{"$nulls":7},"SECTION 13.4: STRUCTURAL STEELWORK (SUNDRY ITEMS) AND GRP"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[16698,"13.4","SABS 1200 H","STRUCTURAL STEELWORK (SUNDRY ITEMS) AND GRP"]
[]
[16994,"13.4.1",null,"FENCING"]
[]
[16996,"13.4.1.1",null,"Supply and install double leaf entrance gate complete as per details on EWS Drawing 45004. (Rate to include for supply, fabricate and installation)","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E164 = CHAR(37), F164*G164/100,F164*G164)","v":{"v":0,"d":"0.00"}}]
[]
[16843,"13.4.2",null,"HANDRAILS"]
[]
[16844,"13.4.2.1",null,"Supply and install top/side mounted Stainless Steel Handrail assembly complete with stanchions, bends and ends with chemical anchors","m",{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"$f":"IF(E168 = CHAR(37), F168*G168/100,F168*G168)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":43}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H160:H211)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 13 - MISCELLANEOUS WORKS"]
[{"$nulls":7},"SECTION 13.5: OTHER"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[24185,"13.5",null,"OTHER"]
[]
[24186,"13.5.1",null,"Provisional sum for painting of above ground pipework with UV stable coating","Prov Sum",{"v":1,"d":"1.00"},{"v":100000,"d":"100,000.00"},{"v":100000,"d":"100,000.00"}]
[]
[24187,"13.5.2",null,"Overheads and Profit on the above item","%",{"$f":"H218","v":{"v":100000,"d":"100,000.00"}},{"v":0,"d":"0.00"},{"$f":"IF(E220 = CHAR(37), F220*G220/100,F220*G220)","v":{"v":0,"d":"0.00"}}]
[]
[24188,"13.5.3",null,"Provisional sum for coating/painting of existing pipework within the TWTW site for ease of identification.","Prov Sum",{"v":1,"d":"1.00"},{"v":100000,"d":"100,000.00"},{"v":100000,"d":"100,000.00"}]
[]
[24189,"13.5.4",null,"Overheads and Profit on the above item","%",{"v":100000,"d":"100,000.00"},{"v":0,"d":"0.00"},{"$f":"IF(E224 = CHAR(37), F224*G224/100,F224*G224)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":45}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H216:H269)","v":{"v":200000,"d":"200,000.00"}}]
[null,"SCHEDULE 13 - MISCELLANEOUS WORKS"]
[{"$nulls":3},"SUMMARY OF SECTIONS"]
[null," ","SECTION","DESCRIPTION",{"$nulls":3},"AMOUNT\n(RAND)"]
[null,null,"13.1","SECTION 13.1: SITE CLEARANCE",{"$nulls":3},{"$f":"H50","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"13.2","SECTION 13.2: GABIONS AND PITCHING",{"$nulls":3},{"$f":"H97","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"13.3","SECTION 13.3: CONCRETE (STRUCTURAL)",{"$nulls":3},{"$f":"H156","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"13.4","SECTION 13.4: STRUCTURAL STEELWORK (SUNDRY ITEMS) AND GRP",{"$nulls":3},{"$f":"H212","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"13.5","SECTION 13.5: OTHER",{"$nulls":3},{"$f":"H270","v":{"v":200000,"d":"200,000.00"}}]
{"$rows_empty":49}
[null,null," Total Carried Forward To Summary Of Schedules"," Total Carried Forward To Summary Of Schedules",{"$nulls":3},{"$f":"SUM(H274:H331)","v":{"v":200000,"d":"200,000.00"}}]

{"sheet":"Schedule 14","index":13,"n_rows":261,"n_cols":8,"rows_kept":261}
["Rate=G","SCHEDULE 14: MECHANICAL EQUIPMENT & ANCILLARY WORKS"]
[{"$nulls":7},"SECTION 14.1: MECHANICAL & PUMP INSTALLATIONS  "]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[22678,"14.1","PSWPE","MECHANICAL EQUIPMENT AND ANCILLARY WORKS"]
[]
[22679,null,null,"Note : All pump pipework, valves, fittings and associated equipment are measured elsewhere"]
[]
[22701,null,null,"Design , supply , manufacture , deliver , offload , install , connect up, test and commission, guarantee and maintaining the pumping plant and associated equipment to EWS  standards and to the relevant SANS, BS or other recognised codes and standards"]
[]
[22680,"14.1.1",null,"Carry out an audit and assessment on the existing Backwash Pumps  and associated motors and provide a detailed report on findings and remedial works required for the Engineers approval.","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E10 = CHAR(37), F10*G10/100,F10*G10)","v":{"v":0,"d":"0.00"}}]
[]
[22727,null,null,"Make safe, disconnect, remove, lift or load , transport and deliver the existing pump sets, motors and associated equipment to EWS Stores and offload as follows :"]
[]
[22732,"14.1.1.1",null,"a) Existing Backwash Recycle Pump","No.",{"v":1,"d":"1.00"},{"v":125,"d":"125.00"},{"v":125,"d":"125.00"}]
[]
[22728,"14.1.1.2",null,"b) Existing sludge pumps - submersible type ","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E16 = CHAR(37), F16*G16/100,F16*G16)","v":{"v":0,"d":"0.00"}}]
[]
[22729,"14.1.1.3",null,"c) Existing sampling pumps","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E18 = CHAR(37), F18*G18/100,F18*G18)","v":{"v":0,"d":"0.00"}}]
[]
[22681,"14.1.2","PS WPE 6, 7, 8, 9 & 10","Design, manufacture , supply and deliver the following new pump sets ( to replace existing ) : "]
[]
[22682,"14.1.2.1",null,"a) Self priming backwash recycle pump ( excluding motor ) , base , coupling , coupling guards, mounting / support frame, belts etc including all sensors as specified complete ( 1 duty, and 1 stand-by ) - duty 55m³/hr @ 5,8m head as specified.","No.",{"v":2,"d":"2.0"},{"v":0,"d":"0.00"},{"$f":"IF(E22 = CHAR(37), F22*G22/100,F22*G22)","v":{"v":0,"d":"0.00"}}]
[]
[22683,"14.1.2.2",null,"b) Submersible sludge pump with motor , coupling , guide rail etc including all sensors as specified complete ( 1 duty, and 1 stand-by ) - duty 34m³/hr @ 6,5m head as specified and supplied by KSB type Amarex NF80-220 or similar and equal approved ","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E24 = CHAR(37), F24*G24/100,F24*G24)","v":{"v":0,"d":"0.00"}}]
[]
[22684,"14.1.3",null,"Install, connect up etc the new pump sets supplied above as follows :"]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H4:H27)","v":{"v":125,"d":"125.00"}}]
[null,"SCHEDULE 14: MECHANICAL EQUIPMENT & ANCILLARY WORKS"]
[{"$nulls":7},"SECTION 14.1: MECHANICAL & PUMP INSTALLATIONS  "]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H28","v":{"v":125,"d":"125.00"}}]
[22685,"14.1.3.1",null,"a) Backwash recycle pump","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E33 = CHAR(37), F33*G33/100,F33*G33)","v":{"v":0,"d":"0.00"}}]
[]
[22686,"14.1.3.2",null,"b) Sludge pump","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E35 = CHAR(37), F35*G35/100,F35*G35)","v":{"v":0,"d":"0.00"}}]
[]
[22687,"14.1.3.3",null,"c) Allow for laser alignment for the self priming backwash recycle pumps supplied above ( provide certificates )","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E37 = CHAR(37), F37*G37/100,F37*G37)","v":{"v":0,"d":"0.00"}}]
[]
[22688,"14.1.4",null,"Allow for the FAT for the above pumps ( backwash recycle pumps and sludge pumps ) ","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E39 = CHAR(37), F39*G39/100,F39*G39)","v":{"v":0,"d":"0.00"}}]
[]
[22699,"14.1.5",null,"Allow for the Engineer and Client to attend the FAT for the above pumps ( to include for flights, travel, car hire , accommodation, meals , entertainment etc ) . Allowance to be made for 3 persons","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E41 = CHAR(37), F41*G41/100,F41*G41)","v":{"v":0,"d":"0.00"}}]
[]
[22730,"14.1.6",null,"Supply, install and connect up the following ancillary equipment :"]
[]
[22689,"14.1.6.1",null,"a) Wika or similar pressure gauges 0 - 500kPA complete with piping, backing board etc","No",{"v":1,"d":"1.0"},{"v":0,"d":"0.00"},{"$f":"IF(E45 = CHAR(37), F45*G45/100,F45*G45)","v":{"v":0,"d":"0.00"}}]
[]
[22691,"14.1.6.2",null,"b) Wika or similar pressure gauges 0 - 1000kPA complete with piping, backing board etc","No",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"$f":"IF(E47 = CHAR(37), F47*G47/100,F47*G47)","v":{"v":0,"d":"0.00"}}]
[]
[22692,"14.1.6.3",null,"c) ½'' BSP sockets with stop-cocks welded on steel pipework","No",{"v":8,"d":"8.00"},{"v":0,"d":"0.00"},{"$f":"IF(E49 = CHAR(37), F49*G49/100,F49*G49)","v":{"v":0,"d":"0.00"}}]
[]
[22693,"14.1.6.4",null,"d) Electronic pressure transmitters and sensors 0-1000kPA pressure rating","No",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E51 = CHAR(37), F51*G51/100,F51*G51)","v":{"v":0,"d":"0.00"}}]
[]
[22694,"14.1.7",null,"SAT - Test and commission the following pump sets on site as supplied above :"]
[]
[22695,"14.1.7.1",null,"a) Backwash Recycle Pump","No",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E55 = CHAR(37), F55*G55/100,F55*G55)","v":{"v":0,"d":"0.00"}}]
[]
[22696,"14.1.7.2",null,"b) Sludge Pump","No",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E57 = CHAR(37), F57*G57/100,F57*G57)","v":{"v":0,"d":"0.00"}}]
[]
[22731,"14.1.8",null,"Design and submit layout drawings of the pump sets and pipework & valve details and layout drawings for each of the pump systems as follows :"]
[]
[22690,"14.1.8.1",null,"a) Backwash Recycle Pump","Sum",{"v":1,"d":"1.0"},{"v":0,"d":"0.00"},{"$f":"IF(E61 = CHAR(37), F61*G61/100,F61*G61)","v":{"v":0,"d":"0.00"}}]
[]
[22697,"14.1.8.2",null,"b) Sludge Pump","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E63 = CHAR(37), F63*G63/100,F63*G63)","v":{"v":0,"d":"0.00"}}]
[]
[22698,"14.1.8.3",null,"Design and submit technical specifications and detailed dimensioned drawings for all the pump sets supplied above","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E65 = CHAR(37), F65*G65/100,F65*G65)","v":{"v":0,"d":"0.00"}}]
[]
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H32:H66)","v":{"v":125,"d":"125.00"}}]
[null,"SCHEDULE 14: MECHANICAL EQUIPMENT & ANCILLARY WORKS"]
[{"$nulls":7},"SECTION 14.2: MOTORS & ANCILLARY WORKS"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[23019,"14.2","PS WPE 6 , 7 , 8 & 9","MOTORS & ANCILLARY WORKS"]
[]
[23035,"14.2.1",null,"Supply the following WEG or similar approved 525V motors as specified."]
[]
[23036,"14.2.1.1",null,"Self priming backwash recovery pump ","No.",{"v":2,"d":"2.0"},{"v":0,"d":"0.00"},{"$f":"IF(E75 = CHAR(37), F75*G75/100,F75*G75)","v":{"v":0,"d":"0.00"}}]
[]
[23049,"14.2.2",null,"Install new 525V motors in position including all new galvanised bolts, nuts, washers and relevant ancillary components"]
[]
[23050,"14.2.2.1",null,"Self priming backwash recovery pump ","No.",{"v":2,"d":"2.0"},{"v":0,"d":"0.00"},{"$f":"IF(E79 = CHAR(37), F79*G79/100,F79*G79)","v":{"v":0,"d":"0.00"}}]
[]
[23056,"14.2.3",null,"Connect all motors to the respective pump couplings (couplings/belt drives to be provided with pump)"]
[]
[23057,"14.2.3.1",null,"Self priming backwash recovery pump ","No.",{"v":2,"d":"2.0"},{"v":0,"d":"0.00"},{"$f":"IF(E83 = CHAR(37), F83*G83/100,F83*G83)","v":{"v":0,"d":"0.00"}}]
[]
[23063,"14.2.4",null,"Testing and commissioning of new motors. The commissioning of all new motors are to be completed in conjunction with the MCC and equipment testing. (To be undertaken in accordance with the Contractors commissioning plan)"]
[]
[23064,"14.2.4.1",null,"Self priming backwash recovery pump ","No.",{"v":2,"d":"2.0"},{"v":0,"d":"0.00"},{"$f":"IF(E87 = CHAR(37), F87*G87/100,F87*G87)","v":{"v":0,"d":"0.00"}}]
[]
[23070,"14.2.5",null,"Testing and Commissioning data sheets to be provided for all motors including a summary report","Sum",{"v":1,"d":"1.0"},{"v":0,"d":"0.00"},{"$f":"IF(E89 = CHAR(37), F89*G89/100,F89*G89)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":26}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H71:H115)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 14: MECHANICAL EQUIPMENT & ANCILLARY WORKS"]
[{"$nulls":7},"SECTION 14.3: ELECTRIC ACUATORS"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[22702,"14.3","PS ACT1.1 to PS ACT1.16","ELECTRIC ACTUATORS"]
[]
[22703,null,null,"Manufacture , supply. deliver , off-load and install the following electrical valve actuators as specified and in accordance with the EWS specifications and standards as follows :"]
[]
[22704,"14.3.1",null,"CLARIFIERS - DESLUDGE VALVES"]
[]
[22705,"14.3.1.1",null,"a) Electric actuators to fit DN100 resilient seal gate valves ( torque requirement to suit valve )","No",{"v":6,"d":"6.0"},{"v":0,"d":"0.00"},{"$f":"IF(E126 = CHAR(37), F126*G126/100,F126*G126)","v":{"v":0,"d":"0.00"}}]
[]
[22706,"14.3.1.2",null,"b) Electric actuators to fit DN350 resilient seal gate valves ( torque requirement to suit valve )","No",{"v":1,"d":"1.0"},{"v":0,"d":"0.00"},{"$f":"IF(E128 = CHAR(37), F128*G128/100,F128*G128)","v":{"v":0,"d":"0.00"}}]
[]
[22707,"14.3.1.3",null,"c) Deliver the above electric actuators to the valve supplier for fitting of the actuators to the valves ","No",{"v":7,"d":"7.0"},{"v":0,"d":"0.00"},{"$f":"IF(E130 = CHAR(37), F130*G130/100,F130*G130)","v":{"v":0,"d":"0.00"}}]
[]
[22708,"14.3.2",null,"FILTERS - BACKWASH & AIR BLOWER VALVES "]
[]
[22709,"14.3.2.1",null,"d) Electric actuators to fit DN200 resilient seal gate valves ( torque requirement to suit valve )","No",{"v":6,"d":"6.0"},{"v":0,"d":"0.00"},{"$f":"IF(E134 = CHAR(37), F134*G134/100,F134*G134)","v":{"v":0,"d":"0.00"}}]
[]
[22710,"14.3.2.2",null,"e) Electric actuators to fit DN300 resilient seal gate valves ( torque requirement to suit valve )","No",{"v":6,"d":"6.0"},{"v":0,"d":"0.00"},{"$f":"IF(E136 = CHAR(37), F136*G136/100,F136*G136)","v":{"v":0,"d":"0.00"}}]
[]
[22711,"14.3.2.3",null,"f) Electric actuators to fit DN350 resilient seal gate valves ( torque requirement to suit valve )","No",{"v":6,"d":"6.0"},{"v":0,"d":"0.00"},{"$f":"IF(E138 = CHAR(37), F138*G138/100,F138*G138)","v":{"v":0,"d":"0.00"}}]
[]
[22712,"14.3.2.4",null,"g) Deliver the above electric actuators to the valve supplier for fitting of the actuators to the valves ","No",{"v":6,"d":"6.0"},{"v":0,"d":"0.00"},{"$f":"IF(E140 = CHAR(37), F140*G140/100,F140*G140)","v":{"v":0,"d":"0.00"}}]
[]
[22713,"14.3.3",null,"Assist the civil or pipework contractor to fit all the above valve actuators and valves to their respective pipework and connect up ","Sum",{"v":1,"d":"1.0"},{"v":0,"d":"0.00"},{"$f":"IF(E142 = CHAR(37), F142*G142/100,F142*G142)","v":{"v":0,"d":"0.00"}}]
[]
[22714,"14.3.4",null,"Provide labelling to all the valve actuators supplied above","Sum",{"v":1,"d":"1.0"},{"v":0,"d":"0.00"},{"$f":"IF(E144 = CHAR(37), F144*G144/100,F144*G144)","v":{"v":0,"d":"0.00"}}]
[]
[22716,"14.3.5",null,"Allow an amount for the FAT for all the above electric valve actuators  :","Sum",{"v":1,"d":"1.0"},{"v":0,"d":"0.00"},{"$f":"IF(E146 = CHAR(37), F146*G146/100,F146*G146)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":7}
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H120:H153)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 14: MECHANICAL EQUIPMENT & ANCILLARY WORKS"]
[{"$nulls":7},"SECTION 14.3: ELECTRIC ACUATORS"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H154","v":{"v":0,"d":"0.00"}}]
[22717,"14.3.6",null,"Allow for the Engineer and Client to attend the FAT for all the above electric valve actuators ( to include for flights, travel, car hire , accommodation, meals , entertainment etc ) . Allowance to be made for 3 persons","Sum",{"v":1,"d":"1.0"},{"v":0,"d":"0.00"},{"$f":"IF(E159 = CHAR(37), F159*G159/100,F159*G159)","v":{"v":0,"d":"0.00"}}]
[]
[22718,"14.3.7",null,"SAT - Test and commission all the electric valve actuators supplied and installed as above","Sum",{"v":1,"d":"1.0"},{"v":0,"d":"0.00"},{"$f":"IF(E161 = CHAR(37), F161*G161/100,F161*G161)","v":{"v":0,"d":"0.00"}}]
[]
[22719,"14.3.8",null,"Provide training for the EWS Tongaat WTW Plant operations and maintenance staff for the entire WTW and pumping and actuator systems  ","Sum",{"v":1,"d":"1.0"},{"v":0,"d":"0.00"},{"$f":"IF(E163 = CHAR(37), F163*G163/100,F163*G163)","v":{"v":0,"d":"0.00"}}]
[]
[22720,"14.3.9",null,"Provide all labels and signs for all the above pumps ","Sum",{"v":1,"d":"1.0"},{"v":0,"d":"0.00"},{"$f":"IF(E165 = CHAR(37), F165*G165/100,F165*G165)","v":{"v":0,"d":"0.00"}}]
[]
[22721,"14.3.10",null,"Allow a provisional sum of R 100 000,00 for any unforeseen work the amounts of which are to be used entirely at the discretion of the Engineer and Client","Prov Sum",{"v":1,"d":"1.0"},{"v":0,"d":"0.00"},{"$f":"IF(E167 = CHAR(37), F167*G167/100,F167*G167)","v":{"v":0,"d":"0.00"}}]
[]
[22722,"14.3.11",null,"Allow for profit and attendance on provisional sum above","%",{"$f":"H167","v":{"v":0,"d":"0.0"}},{"v":0,"d":"0.00"},{"$f":"IF(E169 = CHAR(37), F169*G169/100,F169*G169)","v":{"v":0,"d":"0.00"}}]
[]
[22724,"14.3.12",null,"Any other items the tenderer considers has been omitted and which requires separate pricing as follows :"]
[]
[22725,null,null,"a)"]
[]
[22726,null,null,"b)"]
{"$rows_empty":23}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H158:H198)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 14: MECHANICAL EQUIPMENT & ANCILLARY WORKS"]
[{"$nulls":3},"SUMMARY OF SECTIONS"]
[null," ","SECTION","DESCRIPTION",{"$nulls":3},"AMOUNT\n(RAND)"]
[null,null,"14.1","SECTION 14.1: MECHANICAL & PUMP INSTALLATIONS  ",{"$nulls":3},{"$f":"H67","v":{"v":125,"d":"125.00"}}]
[]
[null,null,"14.2","SECTION 14.2: MOTORS & ANCILLARY WORKS",{"$nulls":3},{"$f":"H116","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"14.3","SECTION 14.3: ELECTRIC ACUATORS",{"$nulls":3},{"$f":"H199","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":53}
[null,null," Total Carried Forward To Summary Of Schedules"," Total Carried Forward To Summary Of Schedules",{"$nulls":3},{"$f":"SUM(H203:H260)","v":{"v":125,"d":"125.00"}}]

{"sheet":"Schedule 15","index":14,"n_rows":1145,"n_cols":8,"rows_kept":1145}
["Rate=G","SCHEDULE 15 - ELECTRICAL & INSTRUMENTATION"]
[{"$nulls":7},"SECTION 15.1: ELECTRICAL & MCC"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[22769,"15.1",null,"MAIN POWER CABLE RETICULATION SYSTEM"]
[]
[22770,null,null,"Note : All items are re-measurable and only items installed or equipment required can be claimed for payment"]
[]
[22771,"15.1.1",null,"CABLES"]
[]
[22772,null,null,"Supply , installation and termination of copper PVC/SWA/PVC/ECC cables per SANS 1507."]
[]
[22773,null,null,"Laid in ducts, trenches, sleeves, horizontal racks or vertical ducts. Rates shall include the supply and fixing of supports with regard to installation of cables complete. Rates shall include PVC cable ties as required including termination. Trenching measured elsewhere "]
[]
[22774,null,"PS ECI 11","Supply Cables PVC/SWA/PVC/ECC cables per SANS 1507"]
[]
[22775,"15.1.1.1",null,"(a) 1.5mm² x 3 core ECC","m",{"v":400,"d":"400.0"},{"v":0,"d":"0.00"},{"$f":"IF(E16 = CHAR(37), F16*G16/100,F16*G16)","v":{"v":0,"d":"0.00"}}]
[]
[22776,"15.1.1.2",null,"(b) 1.5mm² x 4 Core ECC","m",{"v":450,"d":"450.0"},{"v":0,"d":"0.00"},{"$f":"IF(E18 = CHAR(37), F18*G18/100,F18*G18)","v":{"v":0,"d":"0.00"}}]
[]
[22777,"15.1.1.3",null,"(c) 1.5mm² x 14 core ECC","m",{"v":150,"d":"150.0"},{"v":0,"d":"0.00"},{"$f":"IF(E20 = CHAR(37), F20*G20/100,F20*G20)","v":{"v":0,"d":"0.00"}}]
[]
[22778,"15.1.1.4",null,"(d) 2,5mm² x 4 core ECC","m",{"v":1600,"d":"1,600.0"},{"v":0,"d":"0.00"},{"$f":"IF(E22 = CHAR(37), F22*G22/100,F22*G22)","v":{"v":0,"d":"0.00"}}]
[]
[22779,"15.1.1.5",null,"(e)  6mm² x 3 core ECC","m",{"v":375,"d":"375.0"},{"v":0,"d":"0.00"},{"$f":"IF(E24 = CHAR(37), F24*G24/100,F24*G24)","v":{"v":0,"d":"0.00"}}]
[]
[22780,"15.1.1.6",null,"(f) 10mm² x 3 core ECC","m",{"v":160,"d":"160.0"},{"v":0,"d":"0.00"},{"$f":"IF(E26 = CHAR(37), F26*G26/100,F26*G26)","v":{"v":0,"d":"0.00"}}]
[]
[22781,"15.1.1.7",null,"(g) 16mm² x 2 core ECC","m",{"v":70,"d":"70.0"},{"v":0,"d":"0.00"},{"$f":"IF(E28 = CHAR(37), F28*G28/100,F28*G28)","v":{"v":0,"d":"0.00"}}]
[]
[22782,"15.1.1.8",null,"(h) 25mm² x 4 core ECC","m",{"v":75,"d":"75.0"},{"v":0,"d":"0.00"},{"$f":"IF(E30 = CHAR(37), F30*G30/100,F30*G30)","v":{"v":0,"d":"0.00"}}]
[]
[22733,"15.1.1.9",null,"(i)  35mm² x 4 core ECC","m",{"v":150,"d":"150.0"},{"v":0,"d":"0.00"},{"$f":"IF(E32 = CHAR(37), F32*G32/100,F32*G32)","v":{"v":0,"d":"0.00"}}]
[]
[22734,"15.1.1.10",null,"(j) 150mm² x 4 core ECC","m",{"v":100,"d":"100.0"},{"v":0,"d":"0.00"},{"$f":"IF(E34 = CHAR(37), F34*G34/100,F34*G34)","v":{"v":0,"d":"0.00"}}]
[]
[25372,"15.1.1.11",null,"k) 4mm² x BECW","m",{"v":250,"d":"250.00"},{"v":0,"d":"0.00"},{"$f":"IF(E36 = CHAR(37), F36*G36/100,F36*G36)","v":{"v":0,"d":"0.00"}}]
[]
[25373,"15.1.1.12",null,"l) 6mm² x BECW","m",{"v":150,"d":"150.00"},{"v":0,"d":"0.00"},{"$f":"IF(E38 = CHAR(37), F38*G38/100,F38*G38)","v":{"v":0,"d":"0.00"}}]
[]
[22735,null,"PS ECI 11","Installation of above supplied PVC/SWA/PVC/ECC cables per SANS 1507 and SANS10142-1 in ducts , sleeves, cable tray etc"]
[]
[22736,"15.1.1.13",null,"(a) 1.5mm² x 3 core ECC","m",{"v":400,"d":"400.0"},{"v":0,"d":"0.00"},{"$f":"IF(E42 = CHAR(37), F42*G42/100,F42*G42)","v":{"v":0,"d":"0.00"}}]
[]
[22737,"15.1.1.14",null,"(b) 1.5mm² x 4 Core ECC","m",{"v":450,"d":"450.0"},{"v":0,"d":"0.00"},{"$f":"IF(E44 = CHAR(37), F44*G44/100,F44*G44)","v":{"v":0,"d":"0.00"}}]
[]
[22738,"15.1.1.15",null,"(c) 1.5mm² x 14 core ECC","m",{"v":150,"d":"150.0"},{"v":0,"d":"0.00"},{"$f":"IF(E46 = CHAR(37), F46*G46/100,F46*G46)","v":{"v":0,"d":"0.00"}}]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H4:H47)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 15 - ELECTRICAL & INSTRUMENTATION"]
[{"$nulls":7},"SECTION 15.1: ELECTRICAL & MCC"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H48","v":{"v":0,"d":"0.00"}}]
[22739,"15.1.1.16",null,"(d) 2,5mm² x 4 core ECC","m",{"v":1600,"d":"1,600.0"},{"v":0,"d":"0.00"},{"$f":"IF(E53 = CHAR(37), F53*G53/100,F53*G53)","v":{"v":0,"d":"0.00"}}]
[]
[22740,"15.1.1.17",null,"(e)  6mm² x 3 core ECC","m",{"v":375,"d":"375.0"},{"v":0,"d":"0.00"},{"$f":"IF(E55 = CHAR(37), F55*G55/100,F55*G55)","v":{"v":0,"d":"0.00"}}]
[]
[22741,"15.1.1.18",null,"(f) 10mm² x 3 core ECC","m",{"v":160,"d":"160.0"},{"v":0,"d":"0.00"},{"$f":"IF(E57 = CHAR(37), F57*G57/100,F57*G57)","v":{"v":0,"d":"0.00"}}]
[]
[22742,"15.1.1.19",null,"(g) 16mm² x 2 core ECC","m",{"v":70,"d":"70.0"},{"v":0,"d":"0.00"},{"$f":"IF(E59 = CHAR(37), F59*G59/100,F59*G59)","v":{"v":0,"d":"0.00"}}]
[]
[22743,"15.1.1.20",null,"(h) 25mm² x 4 core ECC","m",{"v":75,"d":"75.0"},{"v":0,"d":"0.00"},{"$f":"IF(E61 = CHAR(37), F61*G61/100,F61*G61)","v":{"v":0,"d":"0.00"}}]
[]
[22744,"15.1.1.21",null,"(i)  35mm² x 4 core ECC","m",{"v":150,"d":"150.0"},{"v":0,"d":"0.00"},{"$f":"IF(E63 = CHAR(37), F63*G63/100,F63*G63)","v":{"v":0,"d":"0.00"}}]
[]
[22745,"15.1.1.22",null,"(j) 150mm² x 4 core ECC","m",{"v":100,"d":"100.0"},{"v":0,"d":"0.00"},{"$f":"IF(E65 = CHAR(37), F65*G65/100,F65*G65)","v":{"v":0,"d":"0.00"}}]
[]
[25374,"15.1.1.23",null,"k) 4mm² x BECW","m",{"v":250,"d":"250.00"},{"v":0,"d":"0.00"},{"$f":"IF(E67 = CHAR(37), F67*G67/100,F67*G67)","v":{"v":0,"d":"0.00"}}]
[]
[25375,"15.1.1.24",null,"l) 6mm² x BECW","m",{"v":150,"d":"150.00"},{"v":0,"d":"0.00"},{"$f":"IF(E69 = CHAR(37), F69*G69/100,F69*G69)","v":{"v":0,"d":"0.00"}}]
[]
[22746,null,"PS ECI 11","Cable Glands : Rates shall include the termination of cables in distribution boards, MCCs , kiosks etc  and equipment per supplier recommended termination detail. To include glands, shrouds, lugs and cable numbers."]
[]
[22747,"15.1.1.25",null,"(a) 1.5mm² x 3 core ECC","No",{"v":80,"d":"80.0"},{"v":0,"d":"0.00"},{"$f":"IF(E73 = CHAR(37), F73*G73/100,F73*G73)","v":{"v":0,"d":"0.00"}}]
[]
[22748,"15.1.1.26",null,"(b) 1.5mm² x 4 Core ECC","No",{"v":90,"d":"90.0"},{"v":0,"d":"0.00"},{"$f":"IF(E75 = CHAR(37), F75*G75/100,F75*G75)","v":{"v":0,"d":"0.00"}}]
[]
[22846,"15.1.1.27",null,"(c) 1.5mm² x 14 core ECC","No",{"v":20,"d":"20.00"},{"v":0,"d":"0.00"},{"$f":"IF(E77 = CHAR(37), F77*G77/100,F77*G77)","v":{"v":0,"d":"0.00"}}]
[]
[22847,"15.1.1.28",null,"(d) 2,5mm² x 4 core ECC","No",{"v":90,"d":"90.00"},{"v":0,"d":"0.00"},{"$f":"IF(E79 = CHAR(37), F79*G79/100,F79*G79)","v":{"v":0,"d":"0.00"}}]
[]
[22848,"15.1.1.29",null,"(e)  6mm² x 3 core ECC","No",{"v":24,"d":"24.00"},{"v":0,"d":"0.00"},{"$f":"IF(E81 = CHAR(37), F81*G81/100,F81*G81)","v":{"v":0,"d":"0.00"}}]
[]
[22849,"15.1.1.30",null,"(f) 10mm² x 3 core ECC","No",{"v":8,"d":"8.00"},{"v":0,"d":"0.00"},{"$f":"IF(E83 = CHAR(37), F83*G83/100,F83*G83)","v":{"v":0,"d":"0.00"}}]
[]
[22850,"15.1.1.31",null,"(g) 16mm² x 2 core ECC","No",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"$f":"IF(E85 = CHAR(37), F85*G85/100,F85*G85)","v":{"v":0,"d":"0.00"}}]
[]
[22851,"15.1.1.32",null,"(h) 25mm² x 4 core ECC","No",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"$f":"IF(E87 = CHAR(37), F87*G87/100,F87*G87)","v":{"v":0,"d":"0.00"}}]
[]
[22852,"15.1.1.33",null,"(i)  35mm² x 4 core ECC","No",{"v":8,"d":"8.00"},{"v":0,"d":"0.00"},{"$f":"IF(E89 = CHAR(37), F89*G89/100,F89*G89)","v":{"v":0,"d":"0.00"}}]
[]
[22853,"15.1.1.34",null,"(j) 150mm² x 4 core ECC","No",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"$f":"IF(E91 = CHAR(37), F91*G91/100,F91*G91)","v":{"v":0,"d":"0.00"}}]
[]
[25376,"15.1.1.35",null,"k) 4mm² x BECW","No",{"v":30,"d":"30.00"},{"v":0,"d":"0.00"},{"$f":"IF(E93 = CHAR(37), F93*G93/100,F93*G93)","v":{"v":0,"d":"0.00"}}]
[]
[25377,"15.1.1.36",null,"l) 6mm² x BECW","No",{"v":30,"d":"30.00"},{"v":0,"d":"0.00"},{"$f":"IF(E95 = CHAR(37), F95*G95/100,F95*G95)","v":{"v":0,"d":"0.00"}}]
[]
[22854,null,null,"TRENCHING etc"]
[]
[22855,"15.1.1.37","SANS1200 DB, PSDB","(a) Trenching  400 wide x 550 deep in pickable to hard ground","m",{"v":120,"d":"120.00"},{"v":0,"d":"0.00"},{"$f":"IF(E99 = CHAR(37), F99*G99/100,F99*G99)","v":{"v":0,"d":"0.00"}}]
[]
[22856,"15.1.1.38",null,"(b) Backfilling of above trenches","m",{"v":120,"d":"120.00"},{"v":0,"d":"0.00"},{"$f":"IF(E101 = CHAR(37), F101*G101/100,F101*G101)","v":{"v":0,"d":"0.00"}}]
[]
[22857,null,null,"Sleeves and accessories (supply and install)"]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H52:H103)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 15 - ELECTRICAL & INSTRUMENTATION"]
[{"$nulls":7},"SECTION 15.1: ELECTRICAL & MCC"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H104","v":{"v":0,"d":"0.00"}}]
[22858,"15.1.1.39",null,"(a) Supply and install cable warning tape","m",{"v":120,"d":"120.00"},{"v":0,"d":"0.00"},{"$f":"IF(E109 = CHAR(37), F109*G109/100,F109*G109)","v":{"v":0,"d":"0.00"}}]
[]
[22859,"15.1.1.40",null,"(b) Concrete cable markers","No.",{"v":8,"d":"8.00"},{"v":575,"d":"575.00"},{"v":4600,"d":"4,600.00"}]
[]
[22860,"15.1.1.41",null,"(c) 110Ø uPVC cable sleeves","m",{"v":20,"d":"20.00"},{"v":0,"d":"0.00"},{"$f":"IF(E113 = CHAR(37), F113*G113/100,F113*G113)","v":{"v":0,"d":"0.00"}}]
[]
[22861,"15.1.1.42",null,"(d) 110 Ø 90º PVC bends","No.",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"$f":"IF(E115 = CHAR(37), F115*G115/100,F115*G115)","v":{"v":0,"d":"0.00"}}]
[]
[22862,"15.1.1.43",null,"(e) Coring 100 Ø holes through 200mm concrete","No.",{"v":8,"d":"8.00"},{"v":0,"d":"0.00"},{"$f":"IF(E117 = CHAR(37), F117*G117/100,F117*G117)","v":{"v":0,"d":"0.00"}}]
[]
[22863,"15.1.1.44",null,"(f) 50 and 75 Ø uPVC cable sleeves","m",{"v":40,"d":"40.00"},{"v":0,"d":"0.00"},{"$f":"IF(E119 = CHAR(37), F119*G119/100,F119*G119)","v":{"v":0,"d":"0.00"}}]
[]
[22864,"15.1.1.45",null,"(g) 50 and 75 Ø 90° PVC bends","No.",{"v":8,"d":"8.00"},{"v":115,"d":"115.00"},{"v":920,"d":"920.00"}]
[]
[22865,"15.1.1.46",null,"(h) 160 dia uPVC cable sleeves","m",{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"$f":"IF(E123 = CHAR(37), F123*G123/100,F123*G123)","v":{"v":0,"d":"0.00"}}]
[]
[22866,"15.1.1.47",null,"(i) 160 dia 90º PVC bends","No",{"v":8,"d":"8.00"},{"v":0,"d":"0.00"},{"$f":"IF(E125 = CHAR(37), F125*G125/100,F125*G125)","v":{"v":0,"d":"0.00"}}]
[]
[22867,"15.1.1.48",null,"(j) Assist civil contractor with setting out and co-ordination of the construction of the sleeves , coring of openings and construction of manholes on site where required","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E127 = CHAR(37), F127*G127/100,F127*G127)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":34}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H108:H161)","v":{"v":5520,"d":"5,520.00"}}]
[null,"SCHEDULE 15 - ELECTRICAL & INSTRUMENTATION"]
[{"$nulls":7},"SECTION 15.2: SMALL POWER DISTRIBUTION BOARDS, MCC & ANCILLARIES"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[22750,"15.2",null,"SMALL POWER DISTRIBUTION BOARDS, MCC & ANCILLARIES"]
[]
[22751,"15.2.1",null,"MOTOR CONTROL PANELS"]
[]
[22752,null,"PS ECI 5","Design, manufacture, supply and install distribution boards, motor control panel etc. complete with doors where applicable, frames, subframes, chassis, fixtures, fittings, circuit breakers spare space, busbar etc. as per specifications and drawings/schematics where provided to SANS 1765 ( to include contractor to provide wiring diagrams and equipment list ) as specified as follows :"]
[]
[22753,"15.2.1.1",null,"c) MCC 05 - Actuated Valve MCC ( Including PLC panel & HMI )","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E172 = CHAR(37), F172*G172/100,F172*G172)","v":{"v":0,"d":"0.00"}}]
[]
[22754,"15.2.1.2",null,"b) MCC 04 - Sludge Pumps MCC","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E174 = CHAR(37), F174*G174/100,F174*G174)","v":{"v":0,"d":"0.00"}}]
[]
[22755,"15.2.1.3",null,"c) MCC 05 - Actuated Valve MCC ( Including PLC panel & HMI )","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E176 = CHAR(37), F176*G176/100,F176*G176)","v":{"v":0,"d":"0.00"}}]
[]
[22756,"15.2.1.4",null,"d) Remote Filter Control Panels 1 - 6","No",{"v":6,"d":"6.00"},{"v":0,"d":"0.00"},{"$f":"IF(E178 = CHAR(37), F178*G178/100,F178*G178)","v":{"v":0,"d":"0.00"}}]
[]
[22839,"15.2.1.5",null,"e) Admin Building DB - A1","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E180 = CHAR(37), F180*G180/100,F180*G180)","v":{"v":0,"d":"0.00"}}]
[]
[22838,"15.2.1.6",null,"f) Gatehouse DB - G1","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E182 = CHAR(37), F182*G182/100,F182*G182)","v":{"v":0,"d":"0.00"}}]
[]
[22841,"15.2.1.7",null,"g) New VSDs and associated control equipment for the existing Backwash Pumps in existing MCC 01  ( replace existing star delta starters )","Sum",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E184 = CHAR(37), F184*G184/100,F184*G184)","v":{"v":0,"d":"0.00"}}]
[]
[22757,"15.2.1.8",null,"h) New VSDs and associated control equipment for the new Backwash Recycle Pumps in the existing MCC 01","Sum",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E186 = CHAR(37), F186*G186/100,F186*G186)","v":{"v":0,"d":"0.00"}}]
[]
[22840,"15.2.1.9",null,"i) Take free issue of the MCC 03 for the Screens & Conveyor and install in position and connect up (free issue by Screens & Conveyor contractor or supplier)","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E188 = CHAR(37), F188*G188/100,F188*G188)","v":{"v":0,"d":"0.00"}}]
[]
[22758,"15.2.1.10",null,"j) UPS for MCC 02 & 05  ( 3 kVA )","Sum",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E190 = CHAR(37), F190*G190/100,F190*G190)","v":{"v":0,"d":"0.00"}}]
[]
[22759,"15.2.1.11","PC ECI 5 ;  PC ECI 7","PLC hardware and HMI for MCC 02 & MCC0 05 as specified under the PLC Specification_Rev 06 ( specification enclosed with the tender) [ incl ethernet/serial links]","Sum",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E192 = CHAR(37), F192*G192/100,F192*G192)","v":{"v":0,"d":"0.00"}}]
[]
[22842,"15.2.1.12",null,"Batteries , UPS , battery charger etc installed in MCC cubicle as specified ( include for anti-theft limit switches on the UPS box, battery box and PLC box)","Sum",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E194 = CHAR(37), F194*G194/100,F194*G194)","v":{"v":0,"d":"0.00"}}]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H166:H194)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 15 - ELECTRICAL & INSTRUMENTATION"]
[{"$nulls":7},"SECTION 15.2: SMALL POWER DISTRIBUTION BOARDS, MCC & ANCILLARIES"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H195","v":{"v":0,"d":"0.00"}}]
[22760,"15.2.1.13",null,"Integrate MCC 03 , MCC 04 and the filter remote control panels to the PLC in MCC 02 & MCC 05","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E200 = CHAR(37), F200*G200/100,F200*G200)","v":{"v":0,"d":"0.00"}}]
[]
[22843,"15.2.1.14",null,"Prepare and submit the hard and soft copies for approval of the FDS specification and  how the PLC software will be implemented ( Provisional item)","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E202 = CHAR(37), F202*G202/100,F202*G202)","v":{"v":0,"d":"0.00"}}]
[]
[22844,"15.2.1.15",null,"Allow for programming of the all PLCs using IEC-61131-3 coding standards ( Ladder Logic or other IEC-61131-3 languages are accepted) as per the PLC Specification _ Rev 06  (Provisional item) ","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E204 = CHAR(37), F204*G204/100,F204*G204)","v":{"v":0,"d":"0.00"}}]
[]
[22761,"15.2.1.16",null,"Allow for Thin Slice testing, FAT’s, SAT’s and Commissioning Stages- As per Quality Control specification. (To be conducted jointly by the EWS Engineers and staff and their representatives)    ","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E206 = CHAR(37), F206*G206/100,F206*G206)","v":{"v":0,"d":"0.00"}}]
[]
[22762,"15.2.1.17",null,"Allow for all PLC & HMI Quality Control as per PLC Specification_ Rev 06 ","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E208 = CHAR(37), F208*G208/100,F208*G208)","v":{"v":0,"d":"0.00"}}]
[]
[22763,"15.2.1.18",null,"Allow a sum for all the PLC licenses , including all profit and attendance","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E210 = CHAR(37), F210*G210/100,F210*G210)","v":{"v":0,"d":"0.00"}}]
[]
[22764,"15.2.1.19",null,"Allow a provisional sum of R 75 000,00 for PLC OEM Training  in terms of PLC programming to EWS staff members at the programmer's offices and which is clearly defined in terms of structure and method and on site training","Prov Sum",{"v":1,"d":"1.00"},{"v":75000,"d":"75,000.00"},{"v":75000,"d":"75,000.00"}]
[]
[25378,"15.2.1.20",null,"Allow for three(3) changes on the PLC and HMI software","Sum",{"v":3,"d":"3.00"},{"v":0,"d":"0.00"},{"$f":"IF(E214 = CHAR(37), F214*G214/100,F214*G214)","v":{"v":0,"d":"0.00"}}]
[]
[22765,"15.2.1.21",null,"Allow a sum of R 350 000,00 for the modifications of the existing MCC 01 and the pumps remote control panel in the ex pump station","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E216 = CHAR(37), F216*G216/100,F216*G216)","v":{"v":0,"d":"0.00"}}]
[]
[22766,"15.2.1.22",null,"Allow for profit and attendance on provisional sum above","%",{"$f":"H216","v":{"v":0,"d":"0.00"}},{"v":0,"d":"0.00"},{"$f":"IF(E218 = CHAR(37), F218*G218/100,F218*G218)","v":{"v":0,"d":"0.00"}}]
[]
[22767,"15.2.1.23","PS ECI 23","Allow a sum to prepare wiring diagrams and component lists for comment and approval for all MCC's, electrical panels, DB's etc. supplied above. ","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E220 = CHAR(37), F220*G220/100,F220*G220)","v":{"v":0,"d":"0.00"}}]
[]
[]
[]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H199:H224)","v":{"v":75000,"d":"75,000.00"}}]
[null,"SCHEDULE 15 - ELECTRICAL & INSTRUMENTATION"]
[{"$nulls":7},"SECTION 15.2: SMALL POWER DISTRIBUTION BOARDS, MCC & ANCILLARIES"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H225","v":{"v":75000,"d":"75,000.00"}}]
[22768,"15.2.1.24",null,"Allow an amount for the Engineers and Client costs to attend the FAT for all the above MCCs, control panels and DBs etc ","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E230 = CHAR(37), F230*G230/100,F230*G230)","v":{"v":0,"d":"0.00"}}]
[]
[22783,"15.2.1.25","PS ECI 23","Allow a sum to prepare the FDS, P & ID diagrams, I/O lists and wiring diagrams, instrument loop diagarms, cable schedule and block diagrams, network and process diagrams  etc complete for all MCCs & DBs, control , automation and PLC systems ,etc supplied above  as specified for the entire project including all for all pump stations ","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E232 = CHAR(37), F232*G232/100,F232*G232)","v":{"v":0,"d":"0.00"}}]
[]
[22879,"15.2.2",null,"CABLE TRAYS & ACCESSORIES"]
[]
[22880,null,"PS ECI 11","Supply and installation of heavy duty hot dipped galvanized perforated cable tray with 76mm high turn including splicers etc. The rate shall include for the fixing of cable tray against walls in a horizontal position from the soffit above by means of M8mm threaded metal rods hangers with anchor bolts at intervals not exceeding 1000mm."]
[]
[22881,"15.2.2.1",null,"a) 100mm cable trays straight","m",{"v":80,"d":"80.00"},{"v":0,"d":"0.00"},{"$f":"IF(E238 = CHAR(37), F238*G238/100,F238*G238)","v":{"v":0,"d":"0.00"}}]
[]
[22882,"15.2.2.2",null,"b) 100mm cable tray bend and tees","No.",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E240 = CHAR(37), F240*G240/100,F240*G240)","v":{"v":0,"d":"0.00"}}]
[]
[22883,"15.2.2.3",null,"c) 200 mm cable ladder","m",{"v":80,"d":"80.00"},{"v":0,"d":"0.00"},{"$f":"IF(E242 = CHAR(37), F242*G242/100,F242*G242)","v":{"v":0,"d":"0.00"}}]
[]
[22884,"15.2.2.4",null,"d) 200mm cable ladder bends and tees","No.",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E244 = CHAR(37), F244*G244/100,F244*G244)","v":{"v":0,"d":"0.00"}}]
[]
[22885,"15.2.2.5",null,"e) 300mm cable ladder","m",{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"$f":"IF(E246 = CHAR(37), F246*G246/100,F246*G246)","v":{"v":0,"d":"0.00"}}]
[]
[22886,"15.2.2.6",null,"f) 300mm cable ladder bends and tees","No.",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E248 = CHAR(37), F248*G248/100,F248*G248)","v":{"v":0,"d":"0.00"}}]
[]
[22887,"15.2.3",null,"ISOLATORS FOR ANCILLARY EQUIPMENT"]
[]
[22888,null,null,"Supply, installation and connection of weatherproof isolator in IP65 slide extension box complete with box"]
[]
[22889,"15.2.3.1",null,"a) 20 Amp 3 pole","No.",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"$f":"IF(E254 = CHAR(37), F254*G254/100,F254*G254)","v":{"v":0,"d":"0.00"}}]
[]
[22890,"15.2.3.2",null,"b) 30 Amp 3 pole","No.",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"$f":"IF(E256 = CHAR(37), F256*G256/100,F256*G256)","v":{"v":0,"d":"0.00"}}]
[]
[22891,"15.2.3.3",null,"c) Weatherproof 20Amp TP rotary isolator adjacent stirrers, actuators etc","No.",{"v":40,"d":"40.00"},{"v":0,"d":"0.00"},{"$f":"IF(E258 = CHAR(37), F258*G258/100,F258*G258)","v":{"v":0,"d":"0.00"}}]
[]
[22892,"15.2.3.4",null,"d) Emergency Stop buttons + stands corrosion proof s/steel","No.",{"v":8,"d":"8.00"},{"v":0,"d":"0.00"},{"$f":"IF(E260 = CHAR(37), F260*G260/100,F260*G260)","v":{"v":0,"d":"0.00"}}]
[]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H229:H262)","v":{"v":75000,"d":"75,000.00"}}]
[null,"SCHEDULE 15 - ELECTRICAL & INSTRUMENTATION"]
[{"$nulls":7},"SECTION 15.2: SMALL POWER DISTRIBUTION BOARDS, MCC & ANCILLARIES"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H263","v":{"v":75000,"d":"75,000.00"}}]
[22893,"15.2.4",null,"Supply and install the following instrument cabling and terminations. Ethernet cabling to be CAT6E industrial grade"]
[]
[22894,"15.2.4.1",null,"a) 1.5 mm² Twisted pair shielded cables - 6 Core ","m",{"v":1600,"d":"1,600.00"},{"v":0,"d":"0.00"},{"$f":"IF(E270 = CHAR(37), F270*G270/100,F270*G270)","v":{"v":0,"d":"0.00"}}]
[]
[22895,"15.2.4.2",null,"b) 1.5 mm² Twisted pair cables - 6 Core Terminations","No.",{"v":80,"d":"80.00"},{"v":0,"d":"0.00"},{"$f":"IF(E272 = CHAR(37), F272*G272/100,F272*G272)","v":{"v":0,"d":"0.00"}}]
[]
[22896,"15.2.4.3",null,"c) Modbus cabling","m",{"v":100,"d":"100.00"},{"v":0,"d":"0.00"},{"$f":"IF(E274 = CHAR(37), F274*G274/100,F274*G274)","v":{"v":0,"d":"0.00"}}]
[]
[22897,"15.2.4.4",null,"d) Modbus terminations/ends","No.",{"v":8,"d":"8.00"},{"v":0,"d":"0.00"},{"$f":"IF(E276 = CHAR(37), F276*G276/100,F276*G276)","v":{"v":0,"d":"0.00"}}]
[]
[22898,"15.2.4.5",null,"e) Fibre optic cabling 6 pair single mode","m",{"v":100,"d":"100.00"},{"v":0,"d":"0.00"},{"$f":"IF(E278 = CHAR(37), F278*G278/100,F278*G278)","v":{"v":0,"d":"0.00"}}]
[]
[22899,"15.2.4.6",null,"f) Fibre optic cabling terminations/splicing","No.",{"v":8,"d":"8.00"},{"v":0,"d":"0.00"},{"$f":"IF(E280 = CHAR(37), F280*G280/100,F280*G280)","v":{"v":0,"d":"0.00"}}]
[]
[22900,"15.2.4.7",null,"g) Cable baskets - 150mm","m",{"v":20,"d":"20.00"},{"v":0,"d":"0.00"},{"$f":"IF(E282 = CHAR(37), F282*G282/100,F282*G282)","v":{"v":0,"d":"0.00"}}]
[]
[22901,"15.2.4.8",null,"h) Weatherproof termination boxes for WTW instruments  with DIN rail, terminals etc.)","No.",{"v":30,"d":"30.00"},{"v":0,"d":"0.00"},{"$f":"IF(E284 = CHAR(37), F284*G284/100,F284*G284)","v":{"v":0,"d":"0.00"}}]
[]
[22902,"15.2.4.9",null,"i) Weatherproof termination boxes with DIN rail, terminals and surge protection arrestors for flow meters and cabling","No",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"$f":"IF(E286 = CHAR(37), F286*G286/100,F286*G286)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":28}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H267:H314)","v":{"v":75000,"d":"75,000.00"}}]
[null,"SCHEDULE 15 - ELECTRICAL & INSTRUMENTATION"]
[{"$nulls":7},"SECTION 15.3: TELEMETRY"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[22784,"15.3","PS ECI 12","TELEMETRY SYSTEM -WTW & PUMP STATIONS "]
[]
[22785,"15.3.1",null,"Disconnect , remove and deliver the existing telemetry system at the WTW to EWS stores","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E321 = CHAR(37), F321*G321/100,F321*G321)","v":{"v":0,"d":"0.00"}}]
[]
[22786,null,null,"Supply, install , test and commission the following to EWS standards and specifications"]
[]
[22787,"15.3.2",null,"a) Telemetry panel at the WTW ( 1 site + control room )","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E325 = CHAR(37), F325*G325/100,F325*G325)","v":{"v":0,"d":"0.00"}}]
[]
[22788,"15.3.3",null,"a) Telemetry panel at the remote reservoirs ( 5 sites + control room )","Sum",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E327 = CHAR(37), F327*G327/100,F327*G327)","v":{"v":0,"d":"0.00"}}]
[]
[22868,"15.3.4",null,"b) Telemetry RTU , digital radios etc ( 6 sites + control room )","Sum",{"v":6,"d":"6.00"},{"v":0,"d":"0.00"},{"$f":"IF(E329 = CHAR(37), F329*G329/100,F329*G329)","v":{"v":0,"d":"0.00"}}]
[]
[22789,"15.3.5",null,"c) Telemetry batteries - 100A/hr ( 2 per site )","No",{"v":12,"d":"12.00"},{"v":0,"d":"0.00"},{"$f":"IF(E331 = CHAR(37), F331*G331/100,F331*G331)","v":{"v":0,"d":"0.00"}}]
[]
[22790,"15.3.6",null,"d) Webb radio antennae and associated cabling, mounting and accessories etc complete (6 sites + control room - WTW & 5 reservoirs)","Sum",{"v":6,"d":"6.00"},{"v":0,"d":"0.00"},{"$f":"IF(E333 = CHAR(37), F333*G333/100,F333*G333)","v":{"v":0,"d":"0.00"}}]
[]
[22791,"15.3.7",null,"e) DC surge protection and optical isolation between serial devices (6 sites )","Sum",{"v":6,"d":"6.00"},{"v":0,"d":"0.00"},{"$f":"IF(E335 = CHAR(37), F335*G335/100,F335*G335)","v":{"v":0,"d":"0.00"}}]
[]
[22903,"15.3.8",null,"f) Configuration , testing and commissioning of telemetry system and instrumentation ( 6 sites + control room )","Sum",{"v":6,"d":"6.00"},{"v":0,"d":"0.00"},{"$f":"IF(E337 = CHAR(37), F337*G337/100,F337*G337)","v":{"v":0,"d":"0.00"}}]
[]
[22904,"15.3.9",null,"g) Integrate telemetry system to EWS SCADA system at EWS Control Room including all hardware, software and integration between all MCCs , PLCs and telemetry panel ( for WTW & Reservoirs )","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E339 = CHAR(37), F339*G339/100,F339*G339)","v":{"v":0,"d":"0.00"}}]
[]
[22905,"15.3.10",null,"h) Supply wiring diagrams, compliance certificates and hand-over data pack for complete telemetry system ( for WTW and Reservoirs )","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E341 = CHAR(37), F341*G341/100,F341*G341)","v":{"v":0,"d":"0.00"}}]
[]
[22906,"15.3.11",null,"i) Integrate telemetry system to EWS SCADA system at EWS Control Room including all hardware, software and integration between all MCCs , PLCs and telemetry panel ( for  WTW & Reservoirs )","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E343 = CHAR(37), F343*G343/100,F343*G343)","v":{"v":0,"d":"0.00"}}]
[]
[]
[]
[]
[]
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H319:H348)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 15 - ELECTRICAL & INSTRUMENTATION"]
[{"$nulls":7},"SECTION 15.4: INSTRUMENTATION, SCADA & PLC SYSTEM"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[22792,"15.4",null,"INSTRUMENTATION, SCADA & PLC SYSTEM"]
[]
[22793,"15.4.1",null,"INSTRUMENTATION"]
[]
[22794,null,"PS ECI 17 ; PS ECI 27","Instrumentation to be as per drawings, schematics, loop diagrams and to comply with EWS or industry standard specifications. Instrumentation to include all necessary sensors, transmitters, controllers and accessories to provide thorough and accurate analysis/control. All Instrumentation to be MODBUS ready unless otherwise stated. Instrumentation make & model to be same or equivalent and to be approved by the Engineer prior to purchase."]
[]
[22795,"15.4.1.1",null,"a) Ultrasonic flow meter as specified - 400dia with earthing rings complete","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E359 = CHAR(37), F359*G359/100,F359*G359)","v":{"v":0,"d":"0.00"}}]
[]
[22796,"15.4.1.2",null,"b) Siemens or similar approved MR200 or similar and equal approved ultrasonic level transmitter ( 0-10m range ) complete with Siemens Echomax XPS0-101 R sensor , remote transmitter with mounting brackets, mounting arms amd all necessary accessories. ( linked to PLC) ","No",{"v":3,"d":"3.00"},{"v":0,"d":"0.00"},{"$f":"IF(E361 = CHAR(37), F361*G361/100,F361*G361)","v":{"v":0,"d":"0.00"}}]
[]
[22869,"15.4.1.3",null,"c) Limit switch AC/DC or similar approved","No",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E363 = CHAR(37), F363*G363/100,F363*G363)","v":{"v":0,"d":"0.00"}}]
[]
[22870,"15.4.1.4",null,"d) Supply and install the IFM or similar and equal approved  electronic no-flow switches with half inch sockets welded to pump delivery pipe as specified ( for raw water and other pumps )","No",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E365 = CHAR(37), F365*G365/100,F365*G365)","v":{"v":0,"d":"0.00"}}]
[]
[22797,"15.4.1.5",null,"e) Supply and install low level cut-out float switches in sumps with s/s chain, weights etc as specified","No",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E367 = CHAR(37), F367*G367/100,F367*G367)","v":{"v":0,"d":"0.00"}}]
[]
[22798,"15.4.1.6",null,"f) Supply and install level electrodes in sumps for control of pumps and for low level cut-out of pumps as specified","No",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E369 = CHAR(37), F369*G369/100,F369*G369)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":10}
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H353:H379)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 15 - ELECTRICAL & INSTRUMENTATION"]
[{"$nulls":7},"SECTION 15.4: INSTRUMENTATION, SCADA & PLC SYSTEM"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H380","v":{"v":0,"d":"0.00"}}]
[22799,"15.4.1.7","PS ECI 17","g) New on-site SCADA system at the WTW complete including all hardware , PC, printer , software etc complete to comply with EWS specifications and drawings. SCADA package to be fully compatible and integrate with PLC  systems . SCADA & PLC to be compatible and integratible or equivalent and be approved by Engineer / Client prior to purchase. SCADA system to be Geo-SCADA as per EWS specifications ","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E385 = CHAR(37), F385*G385/100,F385*G385)","v":{"v":0,"d":"0.00"}}]
[]
[22800,"15.4.1.8",null,"h) Allow a provisional sum of R 175 000,00 to upgrade and re-programme the existing SCADA system in the EWS Control Room to include the WTW and all the reservoirs sites (by certified system integrator for the equipment supplied).","Prov Sum",{"v":1,"d":"1.00"},{"v":75000,"d":"75,000.00"},{"v":75000,"d":"75,000.00"}]
[]
[22801,"15.4.1.9",null,"i) Allow for profit and attendance on above item","%",{"$f":"H387","v":{"v":75000,"d":"75,000.000"}},{"v":0,"d":"0.00"},{"$f":"IF(E389 = CHAR(37), F389*G389/100,F389*G389)","v":{"v":0,"d":"0.00"}}]
[]
[22802,"15.4.1.10",null,"j) Allow an provisional amount of R 75 000,00 for the modifications of the control systems for the operation of the pumping systems","Prov Sum",{"v":1,"d":"1.00"},{"v":65000,"d":"65,000.00"},{"v":65000,"d":"65,000.00"}]
[]
[22803,"15.4.1.11",null,"k) Allow for profit and attendance on  item above","%",{"$f":"H391","v":{"v":65000,"d":"65,000.00"}},{"v":0,"d":"0.00"},{"$f":"IF(E393 = CHAR(37), F393*G393/100,F393*G393)","v":{"v":0,"d":"0.00"}}]
[]
[22804,"15.4.1.12",null,"l) UPS- 6kVA for SCADA System as specified","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E395 = CHAR(37), F395*G395/100,F395*G395)","v":{"v":0,"d":"0.00"}}]
[]
[22805,"15.4.1.13",null,"m) Allow a sum for a PLC/SCADA System Integrator for programming of the all the new PLCs and for the new SCADA systems at WTW  Control Room","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E397 = CHAR(37), F397*G397/100,F397*G397)","v":{"v":0,"d":"0.00"}}]
[]
[22806,"15.4.2",null,"TRANSFORMER "]
[]
[22871,"15.4.2.1",null,"a) Supply , deliver to site and off-load the new 200kVA  525/400 Volt transformer as specified ","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E401 = CHAR(37), F401*G401/100,F401*G401)","v":{"v":0,"d":"0.00"}}]
[]
[22872,"15.4.2.2",null,"b) Install in position and connect up the new transformer ","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E403 = CHAR(37), F403*G403/100,F403*G403)","v":{"v":0,"d":"0.00"}}]
[]
[22873,"15.4.2.3",null,"c) Test and commission the new transformer ","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E405 = CHAR(37), F405*G405/100,F405*G405)","v":{"v":0,"d":"0.00"}}]
[]
[22874,"15.4.2.4",null,"d) Disconnect , make safe and remove the existing 100kVA 525/400 Volt transformer and deliver to EWS stores","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E407 = CHAR(37), F407*G407/100,F407*G407)","v":{"v":0,"d":"0.00"}}]
[]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H384:H409)","v":{"v":140000,"d":"140,000.00"}}]
[null,"SCHEDULE 15 - ELECTRICAL & INSTRUMENTATION"]
[{"$nulls":7},"SECTION 15.4: INSTRUMENTATION, SCADA & PLC SYSTEM"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H410","v":{"v":140000,"d":"140,000.00"}}]
[22875,"15.4.2.5",null,"e) Provide all drawings, documentation and other details of the new transformer ","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E415 = CHAR(37), F415*G415/100,F415*G415)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":56}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H414:H471)","v":{"v":140000,"d":"140,000.00"}}]
[null,"SCHEDULE 15 - ELECTRICAL & INSTRUMENTATION"]
[{"$nulls":7},"SECTION 15.5: LIGHTNING, SMALL POWER & SOCKET INSTALLATION"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[22807,"15.5","PS ECI 8","LIGHTING, SMALL POWER & SOCKET INSTALLATION"]
[]
[22808,null,null,"Supply and Install the following :"]
[]
[22809,"15.5.1",null,"a) Flush 1 lever light switch","No.",{"v":8,"d":"8.00"},{"v":0,"d":"0.00"},{"$f":"IF(E480 = CHAR(37), F480*G480/100,F480*G480)","v":{"v":0,"d":"0.00"}}]
[]
[22810,"15.5.2",null,"b) Surface 1 lever light switch","No.",{"v":8,"d":"8.00"},{"v":0,"d":"0.00"},{"$f":"IF(E482 = CHAR(37), F482*G482/100,F482*G482)","v":{"v":0,"d":"0.00"}}]
[]
[22811,"15.5.3",null,"c) Flush 16A Switched socket outlet","No.",{"v":16,"d":"16.00"},{"v":0,"d":"0.00"},{"$f":"IF(E484 = CHAR(37), F484*G484/100,F484*G484)","v":{"v":0,"d":"0.00"}}]
[]
[22812,"15.5.4",null,"d) Surface 16A Switched socket outlet","No.",{"v":6,"d":"6.00"},{"v":0,"d":"0.00"},{"$f":"IF(E486 = CHAR(37), F486*G486/100,F486*G486)","v":{"v":0,"d":"0.00"}}]
[]
[22813,"15.5.5",null,"e) 16A Switched socked outlet industrial type surface","No.",{"v":8,"d":"8.00"},{"v":0,"d":"0.00"},{"$f":"IF(E488 = CHAR(37), F488*G488/100,F488*G488)","v":{"v":0,"d":"0.00"}}]
[]
[22814,"15.5.6",null,"f) Weatherproof termination boxes CCG Corruguard or similar for actuated valves and instruments with terminals ","Sum",{"v":8,"d":"8.00"},{"v":0,"d":"0.00"},{"$f":"IF(E490 = CHAR(37), F490*G490/100,F490*G490)","v":{"v":0,"d":"0.00"}}]
[]
[22815,"15.5.7",null,"g) Surface 2 way light switch ","No.",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"$f":"IF(E492 = CHAR(37), F492*G492/100,F492*G492)","v":{"v":0,"d":"0.00"}}]
[]
[22816,"15.5.8",null,"h) 20A DP 2 pole isolators for air-conditioning units and extract fans.","No.",{"v":8,"d":"8.00"},{"v":0,"d":"0.00"},{"$f":"IF(E494 = CHAR(37), F494*G494/100,F494*G494)","v":{"v":0,"d":"0.00"}}]
[]
[22817,"15.5.9",null,"i) 32 TP +N and earth welding socket plug surface Ampco or similar approved (cable measured elsewhere)","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E496 = CHAR(37), F496*G496/100,F496*G496)","v":{"v":0,"d":"0.00"}}]
[]
[22818,"15.5.10",null,"j ) 10A DP surface weatherproof rotary lockable isolators","No.",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"$f":"IF(E498 = CHAR(37), F498*G498/100,F498*G498)","v":{"v":0,"d":"0.00"}}]
[]
[22819,"15.5.11",null,"k ) 10A TP surface weatherproof rotary lockable isolators","No.",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"$f":"IF(E500 = CHAR(37), F500*G500/100,F500*G500)","v":{"v":0,"d":"0.00"}}]
[]
[22820,"15.5.12",null,"l) 20A TP +N and earth isolators ","No.",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"$f":"IF(E502 = CHAR(37), F502*G502/100,F502*G502)","v":{"v":0,"d":"0.00"}}]
[]
[22876,"15.5.13",null,"m) Photo cell wall mounted","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E504 = CHAR(37), F504*G504/100,F504*G504)","v":{"v":0,"d":"0.00"}}]
[]
[22877,"15.5.14",null,"n) Heavy duty waterproof motor cable termination box ( lockable ) installed adjacent the motors for easy disconnection of the cables from the motor","No.",{"v":3,"d":"3.00"},{"v":0,"d":"0.00"},{"$f":"IF(E506 = CHAR(37), F506*G506/100,F506*G506)","v":{"v":0,"d":"0.00"}}]
[]
[22878,"15.5.1",null,"PLUG & LIGHT POINTS etc"]
[]
[22821,null,null,"(Flush & surface including conduits, bends, boxes, wiring, cabling etc. complete)"]
[]
[22837,null,null,"Isolate, safely disconnect , remove and transport the following existing damaged electrics to EWS Stores "]
[]
[22909,"15.5.1.1",null,"a) Light fittings ( all types )","No",{"v":12,"d":"12.00"},{"v":0,"d":"0.00"},{"$f":"IF(E514 = CHAR(37), F514*G514/100,F514*G514)","v":{"v":0,"d":"0.00"}}]
[]
[22910,"15.5.1.2",null,"b) Power & plug points , isolators and other power points ( all)","No",{"v":12,"d":"12.00"},{"v":0,"d":"0.00"},{"$f":"IF(E516 = CHAR(37), F516*G516/100,F516*G516)","v":{"v":0,"d":"0.00"}}]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H476:H516)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 15 - ELECTRICAL & INSTRUMENTATION"]
[{"$nulls":7},"SECTION 15.5: LIGHTNING, SMALL POWER & SOCKET INSTALLATION"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H517","v":{"v":0,"d":"0.00"}}]
[22911,"15.5.1.3",null,"c) Level sensors, floats , flow meters, flow switches and other instruments","No",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E522 = CHAR(37), F522*G522/100,F522*G522)","v":{"v":0,"d":"0.00"}}]
[]
[22912,"15.5.1.4",null,"d) Conduits including wiring etc complete","m",{"v":80,"d":"80.00"},{"v":0,"d":"0.00"},{"$f":"IF(E524 = CHAR(37), F524*G524/100,F524*G524)","v":{"v":0,"d":"0.00"}}]
[]
[22913,"15.5.1.5",null,"e) All cables ( for ex transformer , recycle pumps and sludge pumps etc- contractor to ascertain )","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E526 = CHAR(37), F526*G526/100,F526*G526)","v":{"v":0,"d":"0.00"}}]
[]
[22914,"15.5.1.6",null,"f) Disconnect and remove the existing DB in the ex Admin Building","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E528 = CHAR(37), F528*G528/100,F528*G528)","v":{"v":0,"d":"0.00"}}]
[]
[22915,null,null,"Supply and install the following circuit breakers in the existing main panel or MCCs  including making openings and modifying the face plate, connections, wiring etc."]
[]
[22916,"15.5.1.7",null,"a) 10 -20 Amp SP","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E532 = CHAR(37), F532*G532/100,F532*G532)","v":{"v":0,"d":"0.00"}}]
[]
[22917,"15.5.1.8",null,"b) 20 Amp TP","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E534 = CHAR(37), F534*G534/100,F534*G534)","v":{"v":0,"d":"0.00"}}]
[]
[22918,"15.5.1.9",null,"c) 80 - 100 Amp TP","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E536 = CHAR(37), F536*G536/100,F536*G536)","v":{"v":0,"d":"0.00"}}]
[]
[22919,null,null,"Conduits , fittings , wiring, saddles , accessories etc complete for all the structures and building lighting and power points"]
[]
[22920,"15.5.1.10",null,"a) 20 dia PVC conduit","m",{"v":200,"d":"200.00"},{"v":0,"d":"0.00"},{"$f":"IF(E540 = CHAR(37), F540*G540/100,F540*G540)","v":{"v":0,"d":"0.00"}}]
[]
[22921,"15.5.1.11",null,"b) 25 dia PVC conduit","m",{"v":100,"d":"100.00"},{"v":0,"d":"0.00"},{"$f":"IF(E542 = CHAR(37), F542*G542/100,F542*G542)","v":{"v":0,"d":"0.00"}}]
[]
[22922,"15.5.1.12",null,"c) 20 dia galvanised bosal conduit","m",{"v":80,"d":"80.00"},{"v":0,"d":"0.00"},{"$f":"IF(E544 = CHAR(37), F544*G544/100,F544*G544)","v":{"v":0,"d":"0.00"}}]
[]
[22923,"15.5.1.13",null,"d) 25 dia galvanised conduit ","m",{"v":80,"d":"80.00"},{"v":0,"d":"0.00"},{"$f":"IF(E546 = CHAR(37), F546*G546/100,F546*G546)","v":{"v":0,"d":"0.00"}}]
[]
[22924,"15.5.1.14",null,"e) 100 x50 galvanised box with cover ","No.",{"v":40,"d":"40.00"},{"v":0,"d":"0.00"},{"$f":"IF(E548 = CHAR(37), F548*G548/100,F548*G548)","v":{"v":0,"d":"0.00"}}]
[]
[22925,"15.5.1.15",null,"f) 100 x 100 galvanised box with cover","No.",{"v":30,"d":"30.00"},{"v":0,"d":"0.00"},{"$f":"IF(E550 = CHAR(37), F550*G550/100,F550*G550)","v":{"v":0,"d":"0.00"}}]
[]
[22926,"15.5.1.16",null,"g) 20/25 dia round boxes with cover 1-3 way","No.",{"v":40,"d":"40.00"},{"v":0,"d":"0.00"},{"$f":"IF(E552 = CHAR(37), F552*G552/100,F552*G552)","v":{"v":0,"d":"0.00"}}]
[]
[22927,"15.5.1.17",null,"h) 1,5mm² wires","m",{"v":300,"d":"300.00"},{"v":0,"d":"0.00"},{"$f":"IF(E554 = CHAR(37), F554*G554/100,F554*G554)","v":{"v":0,"d":"0.00"}}]
[]
[22928,"15.5.1.18",null,"i) 2,5mm² wires","m",{"v":180,"d":"180.00"},{"v":0,"d":"0.00"},{"$f":"IF(E556 = CHAR(37), F556*G556/100,F556*G556)","v":{"v":0,"d":"0.00"}}]
[]
[22929,"15.5.1.19",null,"j) 4mm² wires","m",{"v":120,"d":"120.00"},{"v":0,"d":"0.00"},{"$f":"IF(E558 = CHAR(37), F558*G558/100,F558*G558)","v":{"v":0,"d":"0.00"}}]
[]
[22930,"15.5.1.20",null,"k) 16mm² wires","m",{"v":120,"d":"120.00"},{"v":0,"d":"0.00"},{"$f":"IF(E560 = CHAR(37), F560*G560/100,F560*G560)","v":{"v":0,"d":"0.00"}}]
[]
[22931,"15.5.1.21",null,"l) 40 x 40 galvanised trunking with covers fixed to wall or suspended from roof or trusses ","m",{"v":40,"d":"40.00"},{"v":0,"d":"0.00"},{"$f":"IF(E562 = CHAR(37), F562*G562/100,F562*G562)","v":{"v":0,"d":"0.00"}}]
[]
[]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H521:H565)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 15 - ELECTRICAL & INSTRUMENTATION"]
[{"$nulls":7},"SECTION 15.5: LIGHTNING, SMALL POWER & SOCKET INSTALLATION"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H566","v":{"v":0,"d":"0.00"}}]
[22932,null,"PS ECI 8","Supply light fittings / luminaries and poles as specified with lamps ( refer tp project specification for details )"]
[]
[22933,null,null,"All lights by TLF Lighting as follows:"]
[]
[22934,"15.5.1.22",null,"a) Type A - Surface 1,5m 2 Tube 2 x 30W  LED corrosion proof diffuser","No.",{"v":16,"d":"16.00"},{"v":0,"d":"0.00"},{"$f":"IF(E575 = CHAR(37), F575*G575/100,F575*G575)","v":{"v":0,"d":"0.00"}}]
[]
[22935,"15.5.1.23",null,"b) Type B - Surface 1,5m 2 Tube 2x30W LED panel light with VDU louvres ( office type lights ) ","No.",{"v":14,"d":"14.00"},{"v":0,"d":"0.00"},{"$f":"IF(E577 = CHAR(37), F577*G577/100,F577*G577)","v":{"v":0,"d":"0.00"}}]
[]
[22936,"15.5.1.24",null,"c) Type C - Surface Bulkhead Aluminium with decorative bowl/body  1 x 18W LED","No.",{"v":12,"d":"12.00"},{"v":0,"d":"0.00"},{"$f":"IF(E579 = CHAR(37), F579*G579/100,F579*G579)","v":{"v":0,"d":"0.00"}}]
[]
[22937,"15.5.1.25",null,"d) Type D - Floodlight with aluminium body 1 x 100W LED with reflector ","No.",{"v":16,"d":"16.00"},{"v":0,"d":"0.00"},{"$f":"IF(E581 = CHAR(37), F581*G581/100,F581*G581)","v":{"v":0,"d":"0.00"}}]
[]
[22938,"15.5.1.26",null,"e) Type E - 10m spigot with loading hinge HDG steel light pole with CB, spigot etc to accept floodlight ","No.",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"$f":"IF(E583 = CHAR(37), F583*G583/100,F583*G583)","v":{"v":0,"d":"0.00"}}]
[]
[22939,null,null,"Install and connect the light fittings and poles supplied above."]
[]
[22940,"15.5.1.27",null,"a) Type A","No.",{"v":16,"d":"16.00"},{"v":0,"d":"0.00"},{"$f":"IF(E587 = CHAR(37), F587*G587/100,F587*G587)","v":{"v":0,"d":"0.00"}}]
[]
[22941,"15.5.1.28",null,"b) Type B ","No.",{"v":14,"d":"14.00"},{"v":0,"d":"0.00"},{"$f":"IF(E589 = CHAR(37), F589*G589/100,F589*G589)","v":{"v":0,"d":"0.00"}}]
[]
[22942,"15.5.1.29",null,"c) Type C ","No.",{"v":12,"d":"12.00"},{"v":0,"d":"0.00"},{"$f":"IF(E591 = CHAR(37), F591*G591/100,F591*G591)","v":{"v":0,"d":"0.00"}}]
[]
[22943,"15.5.1.30",null,"d) Type D","No.",{"v":16,"d":"16.00"},{"v":0,"d":"0.00"},{"$f":"IF(E593 = CHAR(37), F593*G593/100,F593*G593)","v":{"v":0,"d":"0.00"}}]
[]
[22944,"15.5.1.31",null,"e) Type E light pole","No.",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"$f":"IF(E595 = CHAR(37), F595*G595/100,F595*G595)","v":{"v":0,"d":"0.00"}}]
[]
[22945,null,null,"Cable joints for existing lights or other cables"]
[]
[22946,"15.5.1.32",null,"a) 25mm² x 4C","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E599 = CHAR(37), F599*G599/100,F599*G599)","v":{"v":0,"d":"0.00"}}]
[]
[22947,"15.5.1.33",null,"b) 16mm² x 4C","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E601 = CHAR(37), F601*G601/100,F601*G601)","v":{"v":0,"d":"0.00"}}]
[]
[22948,"15.5.1.34",null,"c) Relocate the existing UPS in the existing Admin Building to the new Control Room in the new Admin Building","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E603 = CHAR(37), F603*G603/100,F603*G603)","v":{"v":0,"d":"0.00"}}]
[]
[22949,"15.5.2",null,"PROVISIONAL SUMS"]
[]
[22950,"15.5.2.1",null,"Allow a provisional sum of R 150 000,00 to modify and upgrade and automate the existing control panels for the Chlorine Dosing and Chemical Dosing systems ","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E607 = CHAR(37), F607*G607/100,F607*G607)","v":{"v":0,"d":"0.00"}}]
[]
[22951,"15.5.2.2",null,"Allow for profit and attendance on above provisional sum","%",{"$f":"H607","v":{"v":0,"d":"0.00"}},{"v":0,"d":"0.00"},{"$f":"IF(E609 = CHAR(37), F609*G609/100,F609*G609)","v":{"v":0,"d":"0.00"}}]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H570:H609)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 15 - ELECTRICAL & INSTRUMENTATION"]
[{"$nulls":7},"SECTION 15.5: LIGHTNING, SMALL POWER & SOCKET INSTALLATION"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H610","v":{"v":0,"d":"0.00"}}]
[22952,"15.5.2.3",null,"Allow a provisional sum of R 350 000,00 to automate , integrate and connect the existing Chlorine Dosing and Chemical Dosing systems to the existing PLC and new SCADA system","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E615 = CHAR(37), F615*G615/100,F615*G615)","v":{"v":0,"d":"0.00"}}]
[]
[22953,"15.5.2.4",null,"Allow for profit and attendance on above provisional sum","%",{"$f":"H615","v":{"v":0,"d":"0.00"}},{"v":0,"d":"0.00"},{"$f":"IF(E617 = CHAR(37), F617*G617/100,F617*G617)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":51}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H614:H668)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 15 - ELECTRICAL & INSTRUMENTATION"]
[{"$nulls":7},"SECTION 15.6: HVAC INSTALLATION"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[22749,"15.6",null," HVAC INSTALLATION"]
[]
[22822,null,null,"Air-conditioning and Ventilation/Extractor Fans:"]
[]
[22823,null,"Refer Drawings \r\nPS ECI 2.2.1.6","Supply and install the following:"]
[]
[22824,"15.6.1",null,"a) Luft or similar and equal approved extract fans type Luft  LPA 500/43F 380Volt 2m³/s with WC500 wall cowl cladding","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E679 = CHAR(37), F679*G679/100,F679*G679)","v":{"v":0,"d":"0.00"}}]
[]
[22825,"15.6.2",null,"b) Create opening in brickwork and side cladding , patch up, waterproof and make good","No.",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E681 = CHAR(37), F681*G681/100,F681*G681)","v":{"v":0,"d":"0.00"}}]
[]
[22826,"15.6.3",null,"c) 12000Btu/hr Samsung or similar approved midwall split aircooled aircon unit (  with indoor evaporator and outdoor condensing unit ) including Bluechem treatment ","No",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E683 = CHAR(37), F683*G683/100,F683*G683)","v":{"v":0,"d":"0.00"}}]
[]
[22827,"15.6.4",null,"d) Refrigerant piping , control cabling and condensate drain pinpig for 12000Btu/hr units ( max 10m each ). Include for PVC trunking","No",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E685 = CHAR(37), F685*G685/100,F685*G685)","v":{"v":0,"d":"0.00"}}]
[]
[22828,"15.6.5",null,"e) 24000Btu/hr Samsung or similar approved midwall split aircooled aircon unit ( with indoor evaporator and outdoor condensing unit ) including Bluechem treatment ","No",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E687 = CHAR(37), F687*G687/100,F687*G687)","v":{"v":0,"d":"0.00"}}]
[]
[22829,"15.6.6",null,"f) Refrigerant piping , control cabling and condensate drain pinpig for 24000Btu/hr units ( max 10m each ). Include for PVC trunking","No",{"v":2,"d":"2.00"},{"v":0,"d":"0.00"},{"$f":"IF(E689 = CHAR(37), F689*G689/100,F689*G689)","v":{"v":0,"d":"0.00"}}]
[]
[22830,"15.6.7",null,"g) Connect all the vent fans and aircon units to their respective electrical isolators or power points","No.",{"v":9,"d":"9.00"},{"v":0,"d":"0.00"},{"$f":"IF(E691 = CHAR(37), F691*G691/100,F691*G691)","v":{"v":0,"d":"0.00"}}]
[]
[22831,"15.6.8",null,"h) Test and commission all the aircon units supplied above","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E693 = CHAR(37), F693*G693/100,F693*G693)","v":{"v":0,"d":"0.00"}}]
[]
[22832,"15.6.9",null,"i) Test and commission the all  ventilation fans supplied above","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E695 = CHAR(37), F695*G695/100,F695*G695)","v":{"v":0,"d":"0.00"}}]
[]
[22833,"15.6.10",null,"j) Issue the compliance certificate for all the air-conditioner and fans electrical installation supplied above","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E697 = CHAR(37), F697*G697/100,F697*G697)","v":{"v":0,"d":"0.00"}}]
[]
[22845,"15.6.11",null,"k) Provide the associated documentation for all the HVAC systems supplied above ( fans and aircon units )","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E699 = CHAR(37), F699*G699/100,F699*G699)","v":{"v":0,"d":"0.00"}}]
[]
[]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H673:H702)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 15 - ELECTRICAL & INSTRUMENTATION"]
[{"$nulls":7},"SECTION 15.6: HVAC INSTALLATION"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H703","v":{"v":0,"d":"0.00"}}]
[22834,"15.6.12",null,"l) Allow a sum of provisional sum of R 50 000,00 for the repairs and modifications to existing extract fans and aircon units ","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E708 = CHAR(37), F708*G708/100,F708*G708)","v":{"v":0,"d":"0.00"}}]
[]
[22835,"15.6.13",null,"m) Allow for profit and attendance for the above provisional sum","%",{"$f":"H708","v":{"v":0,"d":"0.00"}},{"v":0,"d":"0.00"},{"$f":"IF(E710 = CHAR(37), F710*G710/100,F710*G710)","v":{"v":0,"d":"0.00"}}]
[]
[22836,"15.6.14",null,"n) Disconnect , remove and deliver the existing midwall units comprising the indoor and outdoor units complete to EWS stores","No",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"$f":"IF(E712 = CHAR(37), F712*G712/100,F712*G712)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":47}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H707:H759)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 15 - ELECTRICAL & INSTRUMENTATION"]
[{"$nulls":7},"SECTION 15.7: FIRE PROTECTION INSTALLATION"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[22954,"15.7",null,"FIRE PROTECTION INSTALLATION"]
[]
[22990,null,"SANS10400-T","Supply and install the following Fire Protection Equipment:"]
[]
[22991,"15.7.1",null,"a) 9 kg DCP fire extinguisher","No.",{"v":3,"d":"3.00"},{"v":0,"d":"0.00"},{"$f":"IF(E768 = CHAR(37), F768*G768/100,F768*G768)","v":{"v":0,"d":"0.00"}}]
[]
[22992,"15.7.2",null,"b) 5 kg CO2 fire extinguisher","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E770 = CHAR(37), F770*G770/100,F770*G770)","v":{"v":0,"d":"0.00"}}]
[]
[22993,"15.7.3",null,"c) Photo luminescent and standard FE signs","No.",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"$f":"IF(E772 = CHAR(37), F772*G772/100,F772*G772)","v":{"v":0,"d":"0.00"}}]
[]
[22994,"15.7.4",null,"d) Warning - machine starts automatically signage","No",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"$f":"IF(E774 = CHAR(37), F774*G774/100,F774*G774)","v":{"v":0,"d":"0.00"}}]
[]
[22995,"15.7.5",null,"e) Warning - electricity danger and no entry signage ","No",{"v":4,"d":"4.00"},{"v":0,"d":"0.00"},{"$f":"IF(E776 = CHAR(37), F776*G776/100,F776*G776)","v":{"v":0,"d":"0.00"}}]
[]
[22996,"15.7.6",null,"f) Number plate type signage and labels for large pumps","No",{"v":6,"d":"6.00"},{"v":0,"d":"0.00"},{"$f":"IF(E778 = CHAR(37), F778*G778/100,F778*G778)","v":{"v":0,"d":"0.00"}}]
[]
[22997,"15.7.7",null,"g) Lump sum labelling for all other equipment etc complete","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E780 = CHAR(37), F780*G780/100,F780*G780)","v":{"v":0,"d":"0.00"}}]
[]
[22998,"15.7.8",null,"h) All other standard and statutory signage ,labels and notices deemed necessary","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E782 = CHAR(37), F782*G782/100,F782*G782)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":33}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H764:H815)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 15 - ELECTRICAL & INSTRUMENTATION"]
[{"$nulls":7},"SECTION 15.8: OTHER"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[22955,"15.8",null,"OTHER"]
[]
[22988,"15.8.1",null,"a) All other equipment and materials not measured elsewhere but necessary for complete a working installation (specify separately)","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E822 = CHAR(37), F822*G822/100,F822*G822)","v":{"v":0,"d":"0.00"}}]
[]
[22989,"15.8.2",null,"b) Labelling of all switches, switchgear and equipment as specified for all 4 pump stations.","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E824 = CHAR(37), F824*G824/100,F824*G824)","v":{"v":0,"d":"0.00"}}]
[]
[24194,"15.8.3",null,"c) Re-programming of PLC based on updated FDS, PID's and equipment tagging","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E826 = CHAR(37), F826*G826/100,F826*G826)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":46}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H820:H872)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 15 - ELECTRICAL & INSTRUMENTATION"]
[{"$nulls":7},"SECTION 15.9: TESTING AND COMMISSIONING"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[22956,"15.9",null,"TESTING AND COMMISSIONING"]
[]
[22980,"15.9.1","PS ECI 27","Test and commission the complete Electrical & Instrumentation installation as specified for the WTW site all reservoirs comprising the following:","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E879 = CHAR(37), F879*G879/100,F879*G879)","v":{"v":0,"d":"0.00"}}]
[]
[22981,null,null,"a) Develop Site Acceptance Test (SAT) Schedule"]
[]
[22982,null,null,"b) Draft submission to Engineer"]
[]
[22983,null,null,"c) Revisions as required"]
[]
[22984,null,null,"d) Contractor's testing (labour and special test requirements)"]
[]
[22985,null,null,"e) Conduct FAT under Engineer's Supervision"]
[]
[22986,null,null,"f) Conduct SATs under Engineer's Supervision"]
[]
[22987,null,null,"g) Issue Final Certificate of Compliance (COC)"]
{"$rows_empty":34}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H877:H927)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 15 - ELECTRICAL & INSTRUMENTATION"]
[{"$nulls":7},"SECTION 15.10: DOCUMENTATION"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[22957,"15.10","EWS Standards","DOCUMENTATION"]
[]
[22975,"15.10.1",null,"a) Submit As-built Electrical & Instrumentation drawings to the Engineers satisfaction where not measured elsewhere, comprising the following for the WTW site and all reservoirs :","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E934 = CHAR(37), F934*G934/100,F934*G934)","v":{"v":0,"d":"0.00"}}]
[]
[22976,null,null,"1 x full set \"red line\" drawings (hard copy)"]
[]
[22977,null,null,"4 x sets manufacturers and supplier schedules and drawings (hard copy + CD)"]
{"$rows_empty":45}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H932:H983)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 15 - ELECTRICAL & INSTRUMENTATION"]
[{"$nulls":7},"SECTION 15.11: TRAINING"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[22958,"15.11","EWS Standards"," TRAINING"]
[]
[22970,"15.11.1",null,"Provide training to EWS personnel on systems not measured elsewhere for entire M E & I Installation as follows for the WTW site and all reservoirs :","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E990 = CHAR(37), F990*G990/100,F990*G990)","v":{"v":0,"d":"0.00"}}]
[]
[22971,null,null,"a) Skills Transfer : Allow for training of 4 x EWS operations and maintenance members."]
[]
[22972,null,null,"b) Training : Allow for Maintenance team 3 days for 4 people and Operations team 2 days for 4 people."]
[]
[22973,"15.11.2",null,"Provide Training Manuals for entire M E & I Installation not measured elsewhere for critical operation and maintenance of the complete system for the WTW site and all reservoirs","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E996 = CHAR(37), F996*G996/100,F996*G996)","v":{"v":0,"d":"0.00"}}]
[]
[22974,"15.11.3",null,"Test and issue the electrical certificate of compliance (COC) for the entire project. Separate COC's required for each building, structure or installation  ","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E998 = CHAR(37), F998*G998/100,F998*G998)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":35}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H988:H1033)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 15 - ELECTRICAL & INSTRUMENTATION"]
[{"$nulls":7},"SECTION 15.12: GENERAL"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[22959,"15.12","EWS Standards"," GENERAL"]
[]
[22960,"15.12.1",null,"Provisional sum of R175 000,00 for other works as follows : (under Engineer Instruction only)","Prov Sum",{"v":1,"d":"1.00"},{"v":175000,"d":"175,000.00"},{"v":175000,"d":"175,000.00"}]
[]
[22961,null,null,"a) Site acceptance tests (SAT's) by Specialist, Client and Engineering team"]
[]
[22962,null,null,"b) Factory acceptance tests (FAT's) by Contractor, Client and Engineering team"]
[]
[22963,null,null,"Profit and attendance for item above"]
[]
[22964,null,null,"Guarantee and full maintenance of the entire M E & I Installation system for 12 months after handover to the client, comprising the following for the entire WTW site and telemetry systems for the reservoir sites  :"]
[]
[22965,"15.12.2",null,"a) Full list of material and maintenance plan to be provided","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E1050 = CHAR(37), F1050*G1050/100,F1050*G1050)","v":{"v":0,"d":"0.00"}}]
[]
[22966,"15.12.3",null,"b) Material and Labour cost included","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E1052 = CHAR(37), F1052*G1052/100,F1052*G1052)","v":{"v":0,"d":"0.00"}}]
[]
[22967,null,null,"Any other item the tenderer considers has been omitted and which requires pricing as separate items."]
[]
[22968,null,null,"i)"]
[]
[22969,null,null,"ii)"]
{"$rows_empty":25}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H1038:H1083)","v":{"v":175000,"d":"175,000.00"}}]
[null,"SCHEDULE 15 - ELECTRICAL & INSTRUMENTATION"]
[{"$nulls":3},"SUMMARY OF SECTIONS"]
[null," ","SECTION","DESCRIPTION",{"$nulls":3},"AMOUNT\n(RAND)"]
[null,null,"15.1","SECTION 15.1: ELECTRICAL & MCC",{"$nulls":3},{"$f":"H162","v":{"v":5520,"d":"5,520.00"}}]
[]
[null,null,"15.2","SECTION 15.2: SMALL POWER DISTRIBUTION BOARDS, MCC & ANCILLARIES",{"$nulls":3},{"$f":"H315","v":{"v":75000,"d":"75,000.00"}}]
[]
[null,null,"15.3","SECTION 15.3: TELEMETRY",{"$nulls":3},{"$f":"H349","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"15.4","SECTION 15.4: INSTRUMENTATION, SCADA & PLC SYSTEM",{"$nulls":3},{"$f":"H472","v":{"v":140000,"d":"140,000.00"}}]
[]
[null,null,"15.5","SECTION 15.5: LIGHTNING, SMALL POWER & SOCKET INSTALLATION",{"$nulls":3},{"$f":"H669","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"15.6","SECTION 15.6: HVAC INSTALLATION",{"$nulls":3},{"$f":"H760","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"15.7","SECTION 15.7: FIRE PROTECTION INSTALLATION",{"$nulls":3},{"$f":"H816","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"15.8","SECTION 15.8: OTHER",{"$nulls":3},{"$f":"H873","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"15.9","SECTION 15.9: TESTING AND COMMISSIONING",{"$nulls":3},{"$f":"H928","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"15.10","SECTION 15.10: DOCUMENTATION",{"$nulls":3},{"$f":"H984","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"15.11","SECTION 15.11: TRAINING",{"$nulls":3},{"$f":"H1034","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"15.12","SECTION 15.12: GENERAL",{"$nulls":3},{"$f":"H1084","v":{"v":175000,"d":"175,000.00"}}]
{"$rows_empty":34}
[null,null," Total Carried Forward To Summary Of Schedules"," Total Carried Forward To Summary Of Schedules",{"$nulls":3},{"$f":"SUM(H1088:H1144)","v":{"v":395520,"d":"395,520.00"}}]

{"sheet":"Schedule 16","index":15,"n_rows":162,"n_cols":8,"rows_kept":162}
["Rate=G","SCHEDULE 16 - LIGHTNING PROTECTION AND EARTHING INSTALLATION"]
[{"$nulls":7},"SECTION 16.1:  LIGHTNING PROTECTION AND EARTHING INSTALLATION "]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[22999,"16.1","PS ECI 22"," LIGHTNING PROTECTION AND EARTHING INSTALLATION "]
[]
[23000,"16.1.1",null,"Test and carry out the earth resistivity survey and provide results and recommendations ","Sum",{"v":1,"d":"1.0"},{"v":0,"d":"0.00"},{"$f":"IF(E6 = CHAR(37), F6*G6/100,F6*G6)","v":{"v":0,"d":"0.00"}}]
[]
[23001,"16.1.2",null,"Trenching and backfilling for earth ring main or earth mat","m",{"v":160,"d":"160.0"},{"v":0,"d":"0.00"},{"$f":"IF(E8 = CHAR(37), F8*G8/100,F8*G8)","v":{"v":0,"d":"0.00"}}]
[]
[23002,"16.1.3",null,"Trenching and backfilling for earth ring main or earth mat","m",{"v":160,"d":"160.0"},{"v":0,"d":"0.00"},{"$f":"IF(E10 = CHAR(37), F10*G10/100,F10*G10)","v":{"v":0,"d":"0.00"}}]
[]
[23003,"16.1.4",null,"70mm² PVC insulated bonding and earth conductors ","m",{"v":140,"d":"140.0"},{"v":0,"d":"0.00"},{"$f":"IF(E12 = CHAR(37), F12*G12/100,F12*G12)","v":{"v":0,"d":"0.00"}}]
[]
[23004,"16.1.5",null,"2m long copper clad earth electrodes","No",{"v":18,"d":"18.0"},{"v":0,"d":"0.00"},{"$f":"IF(E14 = CHAR(37), F14*G14/100,F14*G14)","v":{"v":0,"d":"0.00"}}]
[]
[23017,"16.1.6",null,"Exothermic welded connections ","No",{"v":20,"d":"20.00"},{"v":0,"d":"0.00"},{"$f":"IF(E16 = CHAR(37), F16*G16/100,F16*G16)","v":{"v":0,"d":"0.00"}}]
[]
[23018,"16.1.7",null,"70mm² terminations  ","No",{"v":40,"d":"40.00"},{"v":0,"d":"0.00"},{"$f":"IF(E18 = CHAR(37), F18*G18/100,F18*G18)","v":{"v":0,"d":"0.00"}}]
[]
[23005,"16.1.8",null,"10mm dia solid aluminium roof terminal conductors saddled to concrete roof","No",{"v":55,"d":"55.0"},{"v":0,"d":"0.00"},{"$f":"IF(E20 = CHAR(37), F20*G20/100,F20*G20)","v":{"v":0,"d":"0.00"}}]
[]
[23006,"16.1.9",null,"Allow for test points in all down conductors","No",{"v":15,"d":"15.0"},{"v":0,"d":"0.00"},{"$f":"IF(E22 = CHAR(37), F22*G22/100,F22*G22)","v":{"v":0,"d":"0.00"}}]
[]
[23007,"16.1.10",null,"10mm dia solid aluminium roof finials at all corners of buildings ","No",{"v":12,"d":"12.0"},{"v":0,"d":"0.00"},{"$f":"IF(E24 = CHAR(37), F24*G24/100,F24*G24)","v":{"v":0,"d":"0.00"}}]
[]
[23008,"16.1.11",null,"Denso wrap to all underground connections ","No",{"v":30,"d":"30.0"},{"v":0,"d":"0.00"},{"$f":"IF(E26 = CHAR(37), F26*G26/100,F26*G26)","v":{"v":0,"d":"0.00"}}]
[]
[23009,"16.1.12",null,"Test and commission the entire lightning protection and earthing installation , provide earth test certificates ( one for each building or structure )","Sum",{"v":1,"d":"1.0"},{"v":0,"d":"0.00"},{"$f":"IF(E28 = CHAR(37), F28*G28/100,F28*G28)","v":{"v":0,"d":"0.00"}}]
[]
[23010,"16.1.13",null,"Allow for labelling and notices for all the earthing systems","Sum",{"v":1,"d":"1.0"},{"v":0,"d":"0.00"},{"$f":"IF(E30 = CHAR(37), F30*G30/100,F30*G30)","v":{"v":0,"d":"0.00"}}]
[]
[23011,"16.1.14",null,"Allow a provisional sum of R 40 000,00 for any un-forseen work to be used entitle at the discretion of the Client or Engineer and for the Engineer to attend the FAT","Sum",{"v":1,"d":"1.0"},{"v":0,"d":"0.00"},{"$f":"IF(E32 = CHAR(37), F32*G32/100,F32*G32)","v":{"v":0,"d":"0.00"}}]
[]
[23012,"16.1.15",null,"Allow for profit and attendance on the above provisional sum","%",{"$f":"H32","v":{"v":0,"d":"0.0"}},{"v":0,"d":"0.00"},{"$f":"IF(E34 = CHAR(37), F34*G34/100,F34*G34)","v":{"v":0,"d":"0.00"}}]
[]
[23013,"16.1.16",null,"Provide associated documentation including all the earth test certificates, compliance certificates , as-built information and drawings and hand-over data packs ","Sum",{"v":1,"d":"1.0"},{"v":0,"d":"0.00"},{"$f":"IF(E36 = CHAR(37), F36*G36/100,F36*G36)","v":{"v":0,"d":"0.00"}}]
[]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H4:H38)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 16 - LIGHTNING PROTECTION AND EARTHING INSTALLATION"]
[{"$nulls":7},"SECTION 16.1:  LIGHTNING PROTECTION AND EARTHING INSTALLATION "]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H39","v":{"v":0,"d":"0.00"}}]
[23014,"16.1.17",null,"Any other item the tenderer considers has been omitted and which requires pricing as separate items.","Sum",{"v":1,"d":"1.0"},{"v":0,"d":"0.00"},{"$f":"IF(E44 = CHAR(37), F44*G44/100,F44*G44)","v":{"v":0,"d":"0.00"}}]
[]
[23015,null,null,"i)"]
[]
[23016,null,null,"ii)"]
{"$rows_empty":52}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H43:H100)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 16 - LIGHTNING PROTECTION AND EARTHING INSTALLATION"]
[{"$nulls":3},"SUMMARY OF SECTIONS"]
[null," ","SECTION","DESCRIPTION",{"$nulls":3},"AMOUNT\n(RAND)"]
[null,null,"16.1","SECTION 16.1:  LIGHTNING PROTECTION AND EARTHING INSTALLATION ",{"$nulls":3},{"$f":"H101","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":56}
[null,null," Total Carried Forward To Summary Of Schedules"," Total Carried Forward To Summary Of Schedules",{"$nulls":3},{"$f":"SUM(H105:H161)","v":{"v":0,"d":"0.00"}}]

{"sheet":"Schedule 17","index":16,"n_rows":488,"n_cols":8,"rows_kept":488}
["Rate=G","SCHEDULE 17: STRUCTURAL REPAIRS/IMPROVEMENTS"]
[{"$nulls":7},"SECTION 17.1: CHAMBERS"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[23812,"17.1",null,"CHAMBERS"]
[]
[23836,"17.1.1",null,"RAW WATER VALVE CHAMBER"]
[]
[23837,null,null,"Surface Repairs"]
[]
[23838,"17.1.1.1",null,"Cleaning and preparation of Concrete Roof Slab and Internal Walls (Water jetting of structure to remove all loose debris and scum)","m²",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E10 = CHAR(37), F10*G10/100,F10*G10)","v":{"v":0,"d":"0.00"}}]
[]
[23839,"17.1.1.2",null,"Crack injection with Sika epoxy resin or similar approved to (tank roof and other areas identified by the Engineer)","m",{"v":6,"d":"6.00"},{"v":0,"d":"0.00"},{"$f":"IF(E12 = CHAR(37), F12*G12/100,F12*G12)","v":{"v":0,"d":"0.00"}}]
[]
[23840,"17.1.1.3",null,"Cracking Filling using SikaGrout-295 Non-Shrink grout or similar approved","m",{"v":6,"d":"6.00"},{"v":0,"d":"0.00"},{"$f":"IF(E14 = CHAR(37), F14*G14/100,F14*G14)","v":{"v":0,"d":"0.00"}}]
[]
[23841,"17.1.1.4",null,"Proprietary cemetitious repair compound Sika 212 or similar approved (Repair systems) to spall areas identified by the Engineer","m²",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E16 = CHAR(37), F16*G16/100,F16*G16)","v":{"v":0,"d":"0.00"}}]
[]
[23842,"17.1.1.5",null,"Curing of repair surfaces by coating the surface with Sika Antisol curing compounds or similar approved to repaired areas","m²",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E18 = CHAR(37), F18*G18/100,F18*G18)","v":{"v":0,"d":"0.00"}}]
[]
[23843,"17.1.1.6",null,"Application of protective treatment (Sika FerroGard 903+, at an application rate of 0.5kg per square meter or similar approved)","m²",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E20 = CHAR(37), F20*G20/100,F20*G20)","v":{"v":0,"d":"0.00"}}]
[]
[23844,"17.1.1.7",null,"Application of flexible waterproofing paint protective layer","m²",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E22 = CHAR(37), F22*G22/100,F22*G22)","v":{"v":0,"d":"0.00"}}]
[]
[23845,"17.1.2",null,"MOTIVE PRV CHAMBER"]
[]
[23846,null,null,"Surface Repairs"]
[]
[23847,"17.1.2.1",null,"Cleaning and preparation of Concrete Roof Slab and Internal Walls (Water jetting of structure to remove all loose debris and scum)","m²",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E28 = CHAR(37), F28*G28/100,F28*G28)","v":{"v":0,"d":"0.00"}}]
[]
[23848,"17.1.2.2",null,"Application of protective treatment (Sika FerroGard 903+, at an application rate of 0.5kg per square meter or similar approved)","m²",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E30 = CHAR(37), F30*G30/100,F30*G30)","v":{"v":0,"d":"0.00"}}]
[]
[23849,"17.1.2.3",null,"Application of flexible waterproofing paint protective layer","m²",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E32 = CHAR(37), F32*G32/100,F32*G32)","v":{"v":0,"d":"0.00"}}]
[]
[23850,"17.1.3",null,"BELVEDERE METER CHAMBER"]
[]
[23851,null,null,"Surface Repairs"]
[]
[]
[]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H4:H40)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 17: STRUCTURAL REPAIRS/IMPROVEMENTS"]
[{"$nulls":7},"SECTION 17.1: CHAMBERS"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H41","v":{"v":0,"d":"0.00"}}]
[23852,"17.1.3.1",null,"Cleaning and preparation of Concrete Roof Slab and Internal Walls (Water jetting of structure to remove all loose debris and scum) and removal of existing paint","m²",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E46 = CHAR(37), F46*G46/100,F46*G46)","v":{"v":0,"d":"0.00"}}]
[]
[23853,"17.1.3.2",null,"Application of protective treatment (Sika FerroGard 903+, at an application rate of 0.5kg per square meter or similar approved)","m²",{"v":7,"d":"7.00"},{"v":0,"d":"0.00"},{"$f":"IF(E48 = CHAR(37), F48*G48/100,F48*G48)","v":{"v":0,"d":"0.00"}}]
[]
[23854,"17.1.3.3",null,"Application of flexible waterproofing paint protective layer (Internal and External Application)","m²",{"v":20,"d":"20.00"},{"v":0,"d":"0.00"},{"$f":"IF(E50 = CHAR(37), F50*G50/100,F50*G50)","v":{"v":0,"d":"0.00"}}]
[]
[23855,null,null,"Miscellaneous"]
[]
[23856,"17.1.3.4",null,"Construct 100mm Concrete Floor Slab 25Mpa inside Meter Chamber","m³",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E54 = CHAR(37), F54*G54/100,F54*G54)","v":{"v":0,"d":"0.00"}}]
[]
[23857,"17.1.4",null,"METCALFE METER CHAMBER"]
[]
[23858,null,null,"Structural Repairs"]
[]
[23859,"17.1.4.1",null,"Remove existing chamber Slab and Replace with new Precast RC Slab 2m x 2m x 150mm thick with new 1.5m x 1.5m Heavy Duty Lockable Galvanized Steel Lid","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E60 = CHAR(37), F60*G60/100,F60*G60)","v":{"v":0,"d":"0.00"}}]
[]
[23860,"17.1.4.2",null,"Repair Chamber Brickwork","m²",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E62 = CHAR(37), F62*G62/100,F62*G62)","v":{"v":0,"d":"0.00"}}]
[]
[23861,null,null,"Surface Repairs"]
[]
[23862,"17.1.4.3",null,"Cleaning and preparation of Concrete Roof Slab and Internal Walls (Water jetting of structure to remove all loose debris and scum) and removal of existing paint","m²",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E66 = CHAR(37), F66*G66/100,F66*G66)","v":{"v":0,"d":"0.00"}}]
[]
[23863,"17.1.4.4",null,"Application of protective treatment (Sika FerroGard 903+, at an application rate of 0.5kg per square meter or similar approved)","m²",{"v":7,"d":"7.00"},{"v":0,"d":"0.00"},{"$f":"IF(E68 = CHAR(37), F68*G68/100,F68*G68)","v":{"v":0,"d":"0.00"}}]
[]
[23864,"17.1.4.5",null,"Application of flexible waterproofing paint protective layer (Internal and External Application)","m²",{"v":20,"d":"20.00"},{"v":0,"d":"0.00"},{"$f":"IF(E70 = CHAR(37), F70*G70/100,F70*G70)","v":{"v":0,"d":"0.00"}}]
[]
[23865,null,null,"Miscellaneous"]
[]
[23866,"17.1.4.6",null,"Construct 100mm Concrete Floor Slab 25Mpa inside Meter Chamber","m³",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E74 = CHAR(37), F74*G74/100,F74*G74)","v":{"v":0,"d":"0.00"}}]
[]
[]
[]
[]
[]
[]
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H45:H80)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 17: STRUCTURAL REPAIRS/IMPROVEMENTS"]
[{"$nulls":7},"SECTION 17.2: CHEMICAL BUILDING"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[23813,"17.2",null,"CHLORINE STORAGE ROOM"]
[]
[23867,"17.2.1",null,"REINFORCED CONCRETE ROOF SLAB"]
[]
[23868,null,null,"Surface Repairs"]
[]
[23869,"17.2.1.1",null,"Cleaning and preparation of Concrete Roof Slab and External Brick Walls (Water jetting of structure to remove all loose debris and scum)","m²",{"v":180,"d":"180.00"},{"v":0,"d":"0.00"},{"$f":"IF(E91 = CHAR(37), F91*G91/100,F91*G91)","v":{"v":0,"d":"0.00"}}]
[]
[23870,"17.2.1.2",null,"Proprietary cemetitious repair compound Sika 212 or similar approved (Repair systems) to spall areas identified by the Engineer","m²",{"v":180,"d":"180.00"},{"v":0,"d":"0.00"},{"$f":"IF(E93 = CHAR(37), F93*G93/100,F93*G93)","v":{"v":0,"d":"0.00"}}]
[]
[23871,"17.2.1.3",null,"Curing of repair surfaces by coating the surface with Sika Antisol curing compounds or similar approved to repaired areas","m²",{"v":180,"d":"180.00"},{"v":0,"d":"0.00"},{"$f":"IF(E95 = CHAR(37), F95*G95/100,F95*G95)","v":{"v":0,"d":"0.00"}}]
[]
[23872,"17.2.1.4",null,"Application of protective treatment (Sika FerroGard 903+, at an application rate of 0.5kg per square meter or similar approved)","m²",{"v":180,"d":"180.00"},{"v":0,"d":"0.00"},{"$f":"IF(E97 = CHAR(37), F97*G97/100,F97*G97)","v":{"v":0,"d":"0.00"}}]
[]
[23873,"17.2.1.5",null,"Application of flexible waterproofing paint protective layer","m²",{"v":180,"d":"180.00"},{"v":0,"d":"0.00"},{"$f":"IF(E99 = CHAR(37), F99*G99/100,F99*G99)","v":{"v":0,"d":"0.00"}}]
[]
[23874,"17.2.2",null,"INTERIOR WALLS(GROUND LEVEL)"]
[]
[23875,null,null,"Surface Repairs"]
[]
[23876,"17.2.2.1",null,"Crack injection with Sika epoxy resin or similar approved to (tank roof and other areas identified by the Engineer)","m",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E105 = CHAR(37), F105*G105/100,F105*G105)","v":{"v":0,"d":"0.00"}}]
[]
[23877,"17.2.2.2",null,"Cracking Filling using SikaGrout-295 Non-Shrink grout or similar approved","m",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E107 = CHAR(37), F107*G107/100,F107*G107)","v":{"v":0,"d":"0.00"}}]
[]
[23878,"17.2.3",null,"INTERIOR CONCRETE ROOF CEILING(GROUND LEVEL)"]
[]
[23879,null,null,"Surface Repairs"]
[]
[23880,"17.2.3.1",null,"Crack injection with Sika epoxy resin or similar approved to (tank roof and other areas identified by the Engineer)","m",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E113 = CHAR(37), F113*G113/100,F113*G113)","v":{"v":0,"d":"0.00"}}]
[]
[23881,"17.2.3.2",null,"Cracking Filling using SikaGrout-295 Non-Shrink grout or similar approved","m",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E115 = CHAR(37), F115*G115/100,F115*G115)","v":{"v":0,"d":"0.00"}}]
[]
[23882,"17.2.4",null,"INTERIOR CONCRETE FLOOR SLAB(GROUND LEVEL)"]
[]
[23883,null,null,"Surface Repairs"]
[]
[]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H85:H122)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 17: STRUCTURAL REPAIRS/IMPROVEMENTS"]
[{"$nulls":7},"SECTION 17.2: CHEMICAL BUILDING"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H123","v":{"v":0,"d":"0.00"}}]
[23884,"17.2.4.1",null,"Crack injection with Sika epoxy resin or similar approved to (tank roof and other areas identified by the Engineer)","m",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E128 = CHAR(37), F128*G128/100,F128*G128)","v":{"v":0,"d":"0.00"}}]
[]
[23885,"17.2.4.2",null,"Cracking Filling using SikaGrout-295 Non-Shrink grout or similar approved","m",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E130 = CHAR(37), F130*G130/100,F130*G130)","v":{"v":0,"d":"0.00"}}]
[]
[23886,"17.2.4.3",null,"Curing of repair surfaces by coating the surface with Sika Antisol curing compounds or similar approved to repaired areas","m²",{"v":180,"d":"180.00"},{"v":0,"d":"0.00"},{"$f":"IF(E132 = CHAR(37), F132*G132/100,F132*G132)","v":{"v":0,"d":"0.00"}}]
[]
[23887,"17.2.4.4",null,"Application of protective treatment (Sika FerroGard 903+, at an application rate of 0.5kg per square meter or similar approved)","m²",{"v":180,"d":"180.00"},{"v":0,"d":"0.00"},{"$f":"IF(E134 = CHAR(37), F134*G134/100,F134*G134)","v":{"v":0,"d":"0.00"}}]
[]
[23888,"17.2.4.5",null,"Replace existing shutter flooring with Steel galvanized graters","m²",{"v":30,"d":"30.00"},{"v":0,"d":"0.00"},{"$f":"IF(E136 = CHAR(37), F136*G136/100,F136*G136)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":40}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H127:H176)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 17: STRUCTURAL REPAIRS/IMPROVEMENTS"]
[{"$nulls":7},"SECTION 17.3: CLARIFIERS 1 - 6"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[23945,"17.3",null,"CLARIFIERS 1 - 6"]
[]
[23946,"17.3.1",null,"CLARIFIERS"]
[]
[23947,null,null,"Allow for draining of raw water, surface cleaning, drying and structural repairs of the clarifiers foundation and floor slab as instructed by the engineer"]
[]
[23951,"17.3.1.1",null,"Structural Repairs","Prov Sum",{"v":1,"d":"1.00"},{"v":100000,"d":"100,000.00"},{"v":100000,"d":"100,000.00"}]
[]
[23952,null,null,"Surface Repairs"]
[]
[23953,"17.3.1.2",null,"Cleaning and preparation of Clarifiers External Walls (Water jetting of structure to remove all loose debris, spall and scum)","m²",{"v":400,"d":"400.00"},{"v":0,"d":"0.00"},{"$f":"IF(E191 = CHAR(37), F191*G191/100,F191*G191)","v":{"v":0,"d":"0.00"}}]
[]
[23954,"17.3.1.3",null,"Proprietary cemetitious repair compound Sika 212 or similar approved (Repair systems) to spall areas identified by the Engineer","m²",{"v":400,"d":"400.00"},{"v":0,"d":"0.00"},{"$f":"IF(E193 = CHAR(37), F193*G193/100,F193*G193)","v":{"v":0,"d":"0.00"}}]
[]
[23955,"17.3.1.4",null,"Curing of repair surfaces by coating the surface with Sika Antisol curing compounds or similar approved to repaired areas","m²",{"v":400,"d":"400.00"},{"v":0,"d":"0.00"},{"$f":"IF(E195 = CHAR(37), F195*G195/100,F195*G195)","v":{"v":0,"d":"0.00"}}]
[]
[23956,"17.3.1.5",null,"Application of protective treatment (Sika FerroGard 903+, at an application rate of 0.5kg per square meter or similar approved)","m²",{"v":400,"d":"400.00"},{"v":0,"d":"0.00"},{"$f":"IF(E197 = CHAR(37), F197*G197/100,F197*G197)","v":{"v":0,"d":"0.00"}}]
[]
[23957,null,null,"Structural Repairs to RC Walls on Clarifiers"]
[]
[23958,"17.3.1.6",null,"Crack injection with Sika epoxy resin or similar approved to (tank roof and other areas identified by the Engineer)","m",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E201 = CHAR(37), F201*G201/100,F201*G201)","v":{"v":0,"d":"0.00"}}]
[]
[23959,"17.3.1.7",null,"Cracking Filling using SikaGrout-295 Non-Shrink grout or similar approved","m",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"$f":"IF(E203 = CHAR(37), F203*G203/100,F203*G203)","v":{"v":0,"d":"0.00"}}]
[]
[23964,"17.3.2",null,"CHANNEL FROM HOW TO CLARIFIER INLETS"]
[]
[23965,"17.3.2.1",null,"Allow for draining of raw water, surface cleaning, drying and structural repairs of the clannel foundation and floor slab as instructed by the engineer","Prov Sum",{"v":1,"d":"1.00"},{"v":100000,"d":"100,000.00"},{"v":100000,"d":"100,000.00"}]
[]
[23966,null,null,"Surface Repairs"]
[]
[23967,"17.3.2.2",null,"Cleaning and preparation of External Walls (Water jetting of structure to remove all loose debris, spall and scum)","m²",{"v":160,"d":"160.00"},{"v":0,"d":"0.00"},{"$f":"IF(E211 = CHAR(37), F211*G211/100,F211*G211)","v":{"v":0,"d":"0.00"}}]
[]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H181:H213)","v":{"v":200000,"d":"200,000.00"}}]
[null,"SCHEDULE 17: STRUCTURAL REPAIRS/IMPROVEMENTS"]
[{"$nulls":7},"SECTION 17.3: CLARIFIERS 1 - 6"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H214","v":{"v":200000,"d":"200,000.00"}}]
[23968,"17.3.2.3",null,"Proprietary cemetitious repair compound Sika 212 or similar approved (Repair systems) to spall areas identified by the Engineer","m²",{"v":160,"d":"160.00"},{"v":0,"d":"0.00"},{"$f":"IF(E219 = CHAR(37), F219*G219/100,F219*G219)","v":{"v":0,"d":"0.00"}}]
[]
[23969,"17.3.2.4",null,"Curing of repair surfaces by coating the surface with Sika Antisol curing compounds or similar approved to repaired areas","m²",{"v":160,"d":"160.00"},{"v":0,"d":"0.00"},{"$f":"IF(E221 = CHAR(37), F221*G221/100,F221*G221)","v":{"v":0,"d":"0.00"}}]
[]
[23970,"17.3.2.5",null,"Application of protective treatment (Sika FerroGard 903+, at an application rate of 0.5kg per square meter or similar approved)","m²",{"v":160,"d":"160.00"},{"v":0,"d":"0.00"},{"$f":"IF(E223 = CHAR(37), F223*G223/100,F223*G223)","v":{"v":0,"d":"0.00"}}]
[]
[23971,null,null,"Structural Repairs"]
[]
[23972,"17.3.2.6",null,"Replace Steel Galvanized Grating and Replace with new GRP Fibre Grating (600mm wide x 1m long)","No.",{"v":60,"d":"60.00"},{"v":0,"d":"0.00"},{"$f":"IF(E227 = CHAR(37), F227*G227/100,F227*G227)","v":{"v":0,"d":"0.00"}}]
[]
[23973,"17.3.3",null,"SIDE CHANNEL FROM CLARIFIER OUTLET TO SAND FILTERS"]
[]
[23974,"17.3.3.1",null,"Allow for draining of raw water, surface cleaning, drying and structural repairs of the clannel foundation and floor slab as instructed by the engineer","Prov Sum",{"v":1,"d":"1.00"},{"v":100000,"d":"100,000.00"},{"v":100000,"d":"100,000.00"}]
[]
[23975,"17.3.3.2",null,"Cleaning and preparation of External Walls (Water jetting of structure to remove all loose debris, spall and scum)","m²",{"v":200,"d":"200.00"},{"v":0,"d":"0.00"},{"$f":"IF(E233 = CHAR(37), F233*G233/100,F233*G233)","v":{"v":0,"d":"0.00"}}]
[]
[23976,"17.3.3.3",null,"Proprietary cemetitious repair compound Sika 212 or similar approved (Repair systems) to spall areas identified by the Engineer","m²",{"v":200,"d":"200.00"},{"v":0,"d":"0.00"},{"$f":"IF(E235 = CHAR(37), F235*G235/100,F235*G235)","v":{"v":0,"d":"0.00"}}]
[]
[23977,"17.3.3.4",null,"Curing of repair surfaces by coating the surface with Sika Antisol curing compounds or similar approved to repaired areas","m²",{"v":200,"d":"200.00"},{"v":0,"d":"0.00"},{"$f":"IF(E237 = CHAR(37), F237*G237/100,F237*G237)","v":{"v":0,"d":"0.00"}}]
[]
[23978,"17.3.3.5",null,"Application of protective treatment (Sika FerroGard 903+, at an application rate of 0.5kg per square meter or similar approved)","m²",{"v":200,"d":"200.00"},{"v":0,"d":"0.00"},{"$f":"IF(E239 = CHAR(37), F239*G239/100,F239*G239)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":11}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H218:H250)","v":{"v":300000,"d":"300,000.00"}}]
[null,"SCHEDULE 17: STRUCTURAL REPAIRS/IMPROVEMENTS"]
[{"$nulls":7},"SECTION 17.4: SAND FILTERS 1 - 5"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[23816,"17.4",null,"SAND FILTERS 1 - 6"]
[]
[23936,"17.4.1",null,"SAND FILTERS "]
[]
[23941,"17.4.1.1",null,"Structural Repairs","Prov Sum",{"v":1,"d":"1.00"},{"v":100000,"d":"100,000.00"},{"v":100000,"d":"100,000.00"}]
{"$rows_empty":54}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H255:H313)","v":{"v":100000,"d":"100,000.00"}}]
[null,"SCHEDULE 17: STRUCTURAL REPAIRS/IMPROVEMENTS"]
[{"$nulls":7},"SECTION 17.6: ADMIN BUILDING"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[23817,"17.5",null," ADMIN BUILDING"]
[]
[23942,null,null,"Surface Repairs"]
[]
[23943,"17.5.1",null,"Crack injection with Sika epoxy resin or similar approved to (tank roof and other areas identified by the Engineer)","m",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E322 = CHAR(37), F322*G322/100,F322*G322)","v":{"v":0,"d":"0.00"}}]
[]
[23944,"17.5.2",null,"Cracking Filling using SikaGrout-295 Non-Shrink grout or similar approved","m",{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"$f":"IF(E324 = CHAR(37), F324*G324/100,F324*G324)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":50}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H318:H374)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 17: STRUCTURAL REPAIRS/IMPROVEMENTS"]
[{"$nulls":7},"SECTION 17.7: OTHER"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[24177,"17.6",null,"OTHER"]
[]
[24178,"17.6.1",null,"Provisional sum for the design, supply, associated ancillary works and installation of new pipework within Clarifiers, including associated supports and brackets achored to clarifier walls.","Prov Sum",{"v":1,"d":"1.00"},{"v":250000,"d":"250,000.00"},{"v":250000,"d":"250,000.00"}]
[]
[24182,"17.6.2",null,"Overheads & profit on above item","%",{"$f":"H381","v":{"v":250000,"d":"250,000.00"}},{"v":0,"d":"0.00"},{"$f":"IF(E383 = CHAR(37), F383*G383/100,F383*G383)","v":{"v":0,"d":"0.00"}}]
[]
[24181,"17.6.3",null,"Provisional sum for the design, supply, associated ancillary works and installation of brickwork within main inlet channel, including associated achorage to channel walls.","Prov Sum",{"v":1,"d":"1.00"},{"v":10000,"d":"10,000.00"},{"v":10000,"d":"10,000.00"}]
[]
[24183,"17.6.4",null,"Overheads & profit on above item","%",{"$f":"H385","v":{"v":10000,"d":"10,000.00"}},{"v":0,"d":"0.00"},{"$f":"IF(E387 = CHAR(37), F387*G387/100,F387*G387)","v":{"v":0,"d":"0.00"}}]
[]
[24179,"17.6.5",null,"Provisional sum for the design, supply, associated ancillary works and installation of an overflow from the clear wate reservoir to the backwash recovery tank.","Prov Sum",{"v":1,"d":"1.00"},{"v":75000,"d":"75,000.00"},{"v":75000,"d":"75,000.00"}]
[]
[24180,"17.6.6",null,"Overheads & profit on above item","%",{"v":10000,"d":"10,000.00"},{"v":0,"d":"0.00"},{"$f":"IF(E391 = CHAR(37), F391*G391/100,F391*G391)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":34}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H379:H425)","v":{"v":335000,"d":"335,000.00"}}]
[null,"SCHEDULE 17: STRUCTURAL REPAIRS/IMPROVEMENTS"]
[{"$nulls":3},"SUMMARY OF SECTIONS"]
[null," ","SECTION","DESCRIPTION",{"$nulls":3},"AMOUNT\n(RAND)"]
[null,null,"17.1","SECTION 17.1: CHAMBERS",{"$nulls":3},{"$f":"H81","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"17.2","SECTION 17.2: CHEMICAL BUILDING",{"$nulls":3},{"$f":"H177","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"17.3","SECTION 17.3: CLARIFIERS 1 - 6",{"$nulls":3},{"$f":"H251","v":{"v":300000,"d":"300,000.00"}}]
[]
[null,null,"17.4","SECTION 17.4: SAND FILTERS 1 - 5",{"$nulls":3},{"$f":"H314","v":{"v":100000,"d":"100,000.00"}}]
[]
[null,null,"17.5","SECTION 17.6: ADMIN BUILDING",{"$nulls":3},{"$f":"H375","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"17.6","SECTION 17.7: OTHER",{"$nulls":3},{"$f":"H426","v":{"v":335000,"d":"335,000.00"}}]
{"$rows_empty":47}
[null,null," Total Carried Forward To Summary Of Schedules"," Total Carried Forward To Summary Of Schedules",{"$nulls":3},{"$f":"SUM(H430:H487)","v":{"v":735000,"d":"735,000.00"}}]

{"sheet":"Schedule 18","index":17,"n_rows":383,"n_cols":8,"rows_kept":383}
["Rate=G","SCHEDULE 18 - CHEMICAL BUILDING"]
[{"$nulls":7},"SECTION 18.1: ALTERATIONS"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[23527,"18.1",null,"ALTERATIONS"]
[]
[23528,null,null,"NOTES:"]
[]
[23529,null,null,"Items described as to be re-used or to be handed over to the Client are to be carefully dismantled where necessary and stacked on site where directed, and the Contractor will be responsible for their removal and storage until required, and shall make good all items missing, damaged or broken at his own expense"]
[]
[23749,null,null,"Alterations to the fabric of existing structures will be executed in stages concurrently with the construction of the new work to ensure that the waterproofing integrity of the structures is maintained."]
[]
[23530,null,null,"Unless otherwise described, no materials from the alterations shall be re-used in any new work without the written approval of the client, with the exception of facing bricks required in filling to openings, etc., which may be re-used if free of cracks and chips and properly cleaned of all mortar"]
[]
[23531,null,null,"The Contractor is to take all dimensions affecting the existing buildings on the site as he will be solely responsible for all new work being to the correct sizes. The Engineer's Representative is to be notified immediately of any discrepancies between the drawings and the existing work and all work affected by these discrepancies is to be suspended until such time as the Engineer's Representative shall authorise its continuance"]
[]
[23535,null,null,"Prices are to include for carting away from site all materials not specifically mentioned as being stored on site for re-use or handed over to the client and all rubbish, debris, etc., arising from the alterations, etc., and for making good all work damaged or disturbed to the approval of the client"]
[]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H4:H18)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 18 - CHEMICAL BUILDING"]
[{"$nulls":7},"SECTION 18.1: ALTERATIONS"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H19","v":{"v":0,"d":"0.00"}}]
[23536,null,null,"Tenderers are to include in pricing for the statutory requirements with regard to the demolition and disposal of asbestos cement material arising from the works"]
[]
[23537,"18.1.1",null,"GENERAL "]
[]
[23538,"18.1.1.1",null,"Allow for protecting all existing work liable to suffer damage (i.e. walls, finishes, floors, windows, etc.) from damage during the building operations, alterations, etc., and make good all work damaged with new material to match existing to the approval of the client","Sum",{"v":1,"d":"1.0"},{"v":0,"d":"0.00"},{"$f":"IF(E28 = CHAR(37), F28*G28/100,F28*G28)","v":{"v":0,"d":"0.00"}}]
[]
[23540,"18.1.2",null,"REMOVAL OF EXISTING WORK "]
[]
[23543,null,null,"Taking out and removing doors, windows, etc., from brickwork to remain (building up or altering opening elsewhere measured)"]
[]
[23683,"18.1.2.1",null,"Hardwood single door and frame not exceeding 2,5m²\r\n","No.",{"v":2,"d":"2.0"},{"v":0,"d":"0.00"},{"$f":"IF(E34 = CHAR(37), F34*G34/100,F34*G34)","v":{"v":0,"d":"0.00"}}]
[]
[23544,"18.1.2.2",null,"Glazed steel window not exceeding 2,5m²","No.",{"v":14,"d":"14.0"},{"v":0,"d":"0.00"},{"$f":"IF(E36 = CHAR(37), F36*G36/100,F36*G36)","v":{"v":0,"d":"0.00"}}]
[]
[23792,"18.1.2.3",null,"Roller Shutter Garage Door","No.",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E38 = CHAR(37), F38*G38/100,F38*G38)","v":{"v":0,"d":"0.00"}}]
[]
[23545,null,null,"Taking out doors, windows, etc including thresholds, sills, etc from brickwork to be demolished and stored for reuse as directed by the Engineer."]
[]
[23547,"18.1.2.4",null,"Provisional Sum for the Removal of applicable items from the building","Prov Sum",{"v":1,"d":"1.0"},{"v":10000,"d":"10,000.00"},{"v":10000,"d":"10,000.00"}]
[]
[23684,"18.1.2.5",null,"Overheads and Profit on the above","%",{"$f":"H42","v":{"v":10000,"d":"10,000.0"}},{"v":0,"d":"0.00"},{"$f":"IF(E44 = CHAR(37), F44*G44/100,F44*G44)","v":{"v":0,"d":"0.00"}}]
[]
[23568,"18.1.3",null,"PREPARATORY WORK TO EXISTING SURFACES "]
[]
[23569,null,null,"Preparatory work to existing surfaces "]
[]
[23572,"18.1.3.1",null,"Remove paint and plaster surface from existing walls","m²",{"v":380,"d":"380.0"},{"v":0,"d":"0.00"},{"$f":"IF(E50 = CHAR(37), F50*G50/100,F50*G50)","v":{"v":0,"d":"0.00"}}]
[]
[]
[]
[]
[]
[]
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H23:H56)","v":{"v":10000,"d":"10,000.00"}}]
[null,"SCHEDULE 18 - CHEMICAL BUILDING"]
[{"$nulls":7},"SECTION 18.3: METALWORK"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[23579,"18.2","SANS 1200 H, PSHA, PACP","METALWORK"]
[]
[23705,"18.2.1","SANS 1200 H","STRUCTURAL STEEL"]
[]
[23725,null,"8.3.7","HANDRAILS"]
[]
[23773,"18.2.1.1",null,"Removal of the existing handrails","m",{"v":20,"d":"20.0"},{"v":0,"d":"0.00"},{"$f":"IF(E67 = CHAR(37), F67*G67/100,F67*G67)","v":{"v":0,"d":"0.00"}}]
[]
[23726,null,"8.3.7 b)","Supply and install stainless steel handrail assembly complete with stanchions, bends and ends with chemical anchors"]
[]
[23727,"18.2.1.2","8.3.7 b) 1)","Horizontal (hand and knee rails)","m",{"v":20,"d":"20.0"},{"v":0,"d":"0.00"},{"$f":"IF(E71 = CHAR(37), F71*G71/100,F71*G71)","v":{"v":0,"d":"0.00"}}]
[]
[23728,"18.2.1.3","8.3.7 b) 2)","Sloping","m",{"v":10,"d":"10.0"},{"v":0,"d":"0.00"},{"$f":"IF(E73 = CHAR(37), F73*G73/100,F73*G73)","v":{"v":0,"d":"0.00"}}]
[]
[23729,"18.2.1.4","8.3.7 b) 3)","Shaped ends and bends","No.",{"v":8,"d":"8.0"},{"v":0,"d":"0.00"},{"$f":"IF(E75 = CHAR(37), F75*G75/100,F75*G75)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":41}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H61:H116)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 18 - CHEMICAL BUILDING"]
[{"$nulls":7},"SECTION 18.3: PLASTERING"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[23580,"18.3","PABR 5.3.1","PLASTERING"]
[]
[23650,"18.3.1",null,"PRICES"]
[]
[23651,null,null,"The prices of mouldings, weathering, skirting, labours, etc. shall include for forming mitres, stops, etc. unless otherwise described"]
[]
[23652,null,null,"The prices of all rendering shall include for working around pipes, balusters, etc"]
[]
[23653,null,null,"Rates for plaster are to include for all filling to and working around electrical conduits, etc., prior to plastering"]
[]
[23654,"18.3.2",null,"SCREEDS"]
[]
[23655,null,null,"Screeds steel trowelled to falls, on concrete"]
[]
[23656,"18.3.2.1",null,"1:3 cement plaster, 30mm min thick on floors and landings","m²",{"v":110,"d":"110.0"},{"v":0,"d":"0.00"},{"$f":"IF(E135 = CHAR(37), F135*G135/100,F135*G135)","v":{"v":0,"d":"0.00"}}]
[]
[23657,"18.3.3",null,"INTERNAL PLASTER"]
[]
[23658,null,null,"One coat cement plaster on brickwork:"]
[]
[23659,"18.3.3.1",null,"Walls","m²",{"v":380,"d":"380.0"},{"v":0,"d":"0.00"},{"$f":"IF(E141 = CHAR(37), F141*G141/100,F141*G141)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":27}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H121:H168)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 18 - CHEMICAL BUILDING"]
[{"$nulls":7},"SECTION 18.4: PAINTING"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[23582,"18.4",null,"PAINTING"]
[]
[23670,"18.4.1",null,"PREPARATORY WORK TO EXISTING WORK"]
[]
[23671,null,null,"Previously painted plastered surfaces:"]
[]
[23672,null,null,"Surfaces shall be thoroughly washed down and allowed to dry completely before any paint is applied. Blistered or peeling paint shall be completely removed and cracks shall be opened, filled with a suitable filler and finished smooth"]
[]
[23673,null,null,"Previously painted metal surfaces:"]
[]
[23674,null,null,"Surfaces shall be thoroughly rubbed and cleaned down. Blistered or peeling paint shall be completely removed down to bare metal"]
[]
[23675,null,null,"Previously painted wood surfaces:"]
[]
[23676,null,null,"Surfaces shall be thoroughly cleaned down. Blistered or peeling paint shall be completely removed and cracks and crevices shall be primed, filled with suitable filler and finished smooth"]
[]
[23677,"18.4.2",null,"PAINTWORK ETC TO PREVIOUSLY PAINTED WORK ON FLOATED PLASTER"]
[]
[23678,null,null,"Prepare and brush surface to remove all loose contaminants and apply and two coats interior quality acrylic emulsion paint"]
[]
[23679,"18.4.2.1",null,"On existing internal walls","m²",{"v":380,"d":"380.0"},{"v":0,"d":"0.00"},{"$f":"IF(E193 = CHAR(37), F193*G193/100,F193*G193)","v":{"v":0,"d":"0.00"}}]
[]
[23680,"18.4.3",null,"PAINTWORK, ETC. TO NEW WORK ON INTERNAL FLOATED PLASTERED SURFACES"]
[]
[23681,null,null,"One coat plaster primer, one undercoat and two finishing coats non drip enamel for interior application"]
[]
[23682,"18.4.3.1",null,"On internal Walls","m²",{"v":380,"d":"380.0"},{"v":0,"d":"0.00"},{"$f":"IF(E199 = CHAR(37), F199*G199/100,F199*G199)","v":{"v":0,"d":"0.00"}}]
[]
[23765,"18.4.4",null,"PAINTWORK, ETC. TO NEW WORK ON INTERNAL CEILING SURFACES"]
[]
[]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H173:H204)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 18 - CHEMICAL BUILDING"]
[{"$nulls":7},"SECTION 18.4: PAINTING"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H205","v":{"v":0,"d":"0.00"}}]
[23766,null,null,"One coat plaster primer, one undercoat and two finishing coats non drip enamel for interior application"]
[]
[23779,"18.4.4.1",null,"On ceiling of existing building","m²",{"v":110,"d":"110.00"},{"v":0,"d":"0.00"},{"$f":"IF(E212 = CHAR(37), F212*G212/100,F212*G212)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":52}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H209:H264)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 18 - CHEMICAL BUILDING"]
[{"$nulls":7},"SECTION 18.5: PROVISIONAL SUMS"]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[23709,"18.5",null,"PROVISIONAL SUMS"]
[]
[23710,null,null,"Windows and Doors"]
[]
[23711,"18.5.1",null,"Replacement of all windows with aluminium windows and replacement of doors","Prov Sum",{"v":1,"d":"1.0"},{"v":50000,"d":"50,000.00"},{"v":50000,"d":"50,000.00"}]
[]
[23712,"18.5.2",null,"Overheads, charges and profit on above item 18.5.1","%",{"$f":"H273","v":{"v":50000,"d":"50,000.0"}},{"v":0,"d":"0.00"},{"$f":"IF(E275 = CHAR(37), F275*G275/100,F275*G275)","v":{"v":0,"d":"0.00"}}]
[]
[23746,null,null,"Furniture"]
[]
[23747,"18.5.3",null,"Supply and install furniture for workshop, storage room and associated rooms","Prov Sum",{"v":1,"d":"1.0"},{"v":50000,"d":"50,000.00"},{"v":50000,"d":"50,000.00"}]
[]
[23748,"18.5.4",null,"Overheads, charges and profit on above item 18.5.3","%",{"$f":"H279","v":{"v":50000,"d":"50,000.0"}},{"v":0,"d":"0.00"},{"$f":"IF(E281 = CHAR(37), F281*G281/100,F281*G281)","v":{"v":0,"d":"0.00"}}]
[]
[23791,null,null,"Ancillary items"]
[]
[23789,"18.5.5",null,"Supply and install ancillary items","Prov Sum",{"v":1,"d":"1.00"},{"v":75000,"d":"75,000.00"},{"v":75000,"d":"75,000.00"}]
[]
[23790,"18.5.6",null,"Overheads, charges and profit on above item 18.5.5","%",{"$f":"H285","v":{"v":75000,"d":"75,000.00"}},{"v":0,"d":"0.00"},{"$f":"IF(E287 = CHAR(37), F287*G287/100,F287*G287)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":33}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H269:H320)","v":{"v":175000,"d":"175,000.00"}}]
[null,"SCHEDULE 18 - CHEMICAL BUILDING"]
[{"$nulls":3},"SUMMARY OF SECTIONS"]
[null," ","SECTION","DESCRIPTION",{"$nulls":3},"AMOUNT\n(RAND)"]
[null,null,"18.1","SECTION 18.1: ALTERATIONS",{"$nulls":3},{"$f":"H57","v":{"v":10000,"d":"10,000.00"}}]
[]
[null,null,"18.2","SECTION 18.2: METALWORK",{"$nulls":3},{"$f":"H117","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"18.3","SECTION 18.3: PLASTERING",{"$nulls":3},{"$f":"H169","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"18.4","SECTION 18.4: PAINTING",{"$nulls":3},{"$f":"H265","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"18.5","SECTION 18.5: PROVISIONAL SUMS",{"$nulls":3},{"$f":"H321","v":{"v":175000,"d":"175,000.00"}}]
{"$rows_empty":49}
[null,null," Total Carried Forward To Summary Of Schedules"," Total Carried Forward To Summary Of Schedules",{"$nulls":3},{"$f":"SUM(H325:H382)","v":{"v":185000,"d":"185,000.00"}}]

{"sheet":"Schedule 19","index":18,"n_rows":146,"n_cols":8,"rows_kept":146}
["Rate=G","SCHEDULE 19: COMMISSIONING & DOCUMENTATION"]
[{"$nulls":7},"SECTION 19.1: COMMISSIOINING & DOCUMENTATION"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[20080,"19.1","PSCOM","COMMISSIONING & DOCUMENTATION"]
[]
[20084,"19.1.1","PSCOM","TONGAAT WTW"]
[]
[20110,"19.1.1.1",null,"Commissioning of the system including the preparation and submission of a comprehensive commissioning plan covering all applicable disciplines and works.","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E8 = CHAR(37), F8*G8/100,F8*G8)","v":{"v":0,"d":"0.00"}}]
[]
[20867,"19.1.1.2","PSCOM 5","Appointment of a commissioning engineer (Professionally Registered) for the entire commissioning period","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E10 = CHAR(37), F10*G10/100,F10*G10)","v":{"v":0,"d":"0.00"}}]
[]
[20111,null,null,"Site testing, commissioning, and adjusting the plant and equipment:"]
[]
[20112,"19.1.1.3",null,"All equipment including checking, starting up, pre- commissioning testing and commissioning of the Works; including reports","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E14 = CHAR(37), F14*G14/100,F14*G14)","v":{"v":0,"d":"0.00"}}]
[]
[20115,"19.1.2","PSCOM","ELECTRICAL & INSTRUMENTATION"]
[]
[20116,"19.1.2.1",null,"Test the entire installation including issue of the Certificate of Compliance certificates in accordance with SANS 10142","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E18 = CHAR(37), F18*G18/100,F18*G18)","v":{"v":0,"d":"0.00"}}]
[]
[20163,"19.1.2.2",null,"Commissioning of the system","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E20 = CHAR(37), F20*G20/100,F20*G20)","v":{"v":0,"d":"0.00"}}]
[]
[20117,"19.1.3","PSCOM","MECHANICAL"]
[]
[20118,"19.1.3.1",null,"Test and commission all mechanical works within the TWTW site boundary (Valves, control valves, actuated valves, dosing systems, etc)","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E24 = CHAR(37), F24*G24/100,F24*G24)","v":{"v":0,"d":"0.00"}}]
[]
[20164,"19.1.3.2",null,"Commissioning of the system","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E26 = CHAR(37), F26*G26/100,F26*G26)","v":{"v":0,"d":"0.00"}}]
[]
[20119,"19.1.4","PSCOM","PROCESS"]
[]
[20120,"19.1.4.1",null,"Test and commission all equipment, process elements and ancillary elements within the TWTW site boundary ","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E30 = CHAR(37), F30*G30/100,F30*G30)","v":{"v":0,"d":"0.00"}}]
[]
[20893,"19.1.4.2",null,"Supply of materials, chemicals and ancillary items for commissioning purposes, the amount is to be determined by the Contractor","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E32 = CHAR(37), F32*G32/100,F32*G32)","v":{"v":0,"d":"0.00"}}]
[]
[20121,"19.1.5",null,"O&M MANUALS, STANDARD OPERATING PROCEDURE'S AND MAINTENANCE SCHEDULES"]
[]
[20892,"19.1.5.1","PS SOP 10","Preparation and submission of Maintenance Schedules","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E36 = CHAR(37), F36*G36/100,F36*G36)","v":{"v":0,"d":"0.00"}}]
[]
[null," Total Carried Forward",{"$nulls":5},{"$f":"SUM(H4:H37)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 19: COMMISSIONING & DOCUMENTATION"]
[{"$nulls":7},"SECTION 19.1: COMMISSIOINING & DOCUMENTATION"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT\n(RAND)"]
[null," Brought Forward",{"$nulls":5},{"$f":"H38","v":{"v":0,"d":"0.00"}}]
[23510,"19.1.5.2","PS SOP","Preparation and submission of Standard Operating Procedures","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E43 = CHAR(37), F43*G43/100,F43*G43)","v":{"v":0,"d":"0.00"}}]
[]
[20123,"19.1.6",null,"FUNCTIONAL DESIGN SPECIFICATIONS"]
[]
[20124,"19.1.6.1",null,"Preparation and submission of the Functional Design Specifications (FDS to be approved prior to any commissioning activities). FDS to be in accordance with EWS specifications. EWS reserve the right to workshop the FDS until the document is accepted by the various M&E, C&I & Process Departments.","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E47 = CHAR(37), F47*G47/100,F47*G47)","v":{"v":0,"d":"0.00"}}]
[]
[20869,"19.1.7",null,"PIPING AND INSTRUMENTATION DIAGRAMS"]
[]
[20870,"19.1.7.1","PS 1.3.1","Preparation of P&ID diagrams for the entire site including all associated plant & equipment. Diagrams in accordance with EWS specifications. To be provided in PDF format, Plant3D and CAD. P&ID diagrams to be provided prior to any commissioning activities.","Sum",{"v":1,"d":"1.00"},{"v":0,"d":"0.00"},{"$f":"IF(E51 = CHAR(37), F51*G51/100,F51*G51)","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":32}
[null," Total Carried Forward To Summary",{"$nulls":5},{"$f":"SUM(H42:H83)","v":{"v":0,"d":"0.00"}}]
[null,"SCHEDULE 19: COMMISSIONING & DOCUMENTATION"]
[{"$nulls":3},"SUMMARY OF SECTIONS"]
[null," ","SECTION","DESCRIPTION",{"$nulls":3},"AMOUNT\n(RAND)"]
[null,null,"19.1","SECTION 19.1: COMMISSIOINING & DOCUMENTATION",{"$nulls":3},{"$f":"H84","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":57}
[null,null," Total Carried Forward To Summary Of Schedules"," Total Carried Forward To Summary Of Schedules",{"$nulls":3},{"$f":"SUM(H88:H145)","v":{"v":0,"d":"0.00"}}]

{"sheet":"Summary Of Schedules","index":19,"n_rows":61,"n_cols":8,"rows_kept":61}
["Rate=G",null,null,"SUMMARY OF SCHEDULES"]
[null," ","SCHEDULE","DESCRIPTION",{"$nulls":3},"AMOUNT\n(RAND)"]
[null,null,"1","SCHEDULE 1 - PRELIMINARY AND GENERAL",{"$nulls":3},{"$f":"'Schedule 1'!H342","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"2","SCHEDULE 2 - PROVISIONAL SUMS",{"$nulls":3},{"$f":"'Schedule 2'!H329","v":{"v":9260000,"d":"9,260,000.00"}}]
[]
[null,null,"3","SCHEDULE 3 - HEAD OF WORKS",{"$nulls":3},{"$f":"'Schedule 3'!H679","v":{"v":750000,"d":"750,000.00"}}]
[]
[null,null,"4","SCHEDULE 4 - FLOCCULATION TANKS",{"$nulls":3},{"$f":"'Schedule 4'!H488","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"5","SCHEDULE 5 - WATERWORKS EQUIPMENT",{"$nulls":3},{"$f":"'Schedule 5'!H299","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"6","SCHEDULE 6 - ADMINISTRATION BUILDING EXTENSION",{"$nulls":3},{"$f":"'Schedule 6'!H1202","v":{"v":480000,"d":"480,000.00"}}]
[]
[null,null,"7","SCHEDULE 7 - SECURITY GUARD HOUSE",{"$nulls":3},{"$f":"'Schedule 7'!H745","v":{"v":67500,"d":"67,500.00"}}]
[]
[null,null,"8","SCHEDULE 8 - BACKWASH, SLUDGE AND BACKWASH RECOVERY SYSTEMS & CHAMBERS",{"$nulls":3},{"$f":"'Schedule 8'!H1164","v":{"v":40000,"d":"40,000.00"}}]
[]
[null,null,"9","SCHEDULE 9 - CLARIFIERS",{"$nulls":3},{"$f":"'Schedule 9'!H212","v":{"v":335000,"d":"335,000.00"}}]
[]
[null,null,"10","SCHEDULE 10 - BACKWASH RECOVERY TANK",{"$nulls":3},{"$f":"'Schedule 10'!H224","v":{"v":15000,"d":"15,000.00"}}]
[]
[null,null,"11","SCHEDULE 11 - ROADS",{"$nulls":3},{"$f":"'Schedule 11'!H293","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"12","SCHEDULE 12 - STORMWATER",{"$nulls":3},{"$f":"'Schedule 12'!H202","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"13","SCHEDULE 13 - MISCELLANEOUS WORKS",{"$nulls":3},{"$f":"'Schedule 13'!H332","v":{"v":200000,"d":"200,000.00"}}]
[]
[null,null,"14","SCHEDULE 14 - MECHANICAL EQUIPMENT & ANCILLARY WORKS",{"$nulls":3},{"$f":"'Schedule 14'!H261","v":{"v":125,"d":"125.00"}}]
[]
[null,null,"15","SCHEDULE 15 - ELECTRICAL & INSTRUMENTATION",{"$nulls":3},{"$f":"'Schedule 15'!H1145","v":{"v":395520,"d":"395,520.00"}}]
[]
[null,null,"16","SCHEDULE 16 - LIGHTNING PROTECTION AND EARTHING INSTALLATION",{"$nulls":3},{"$f":"'Schedule 16'!H162","v":{"v":0,"d":"0.00"}}]
[]
[null,null,"17","SCHEDULE 17: STRUCTURAL REPAIRS/IMPROVEMENTS",{"$nulls":3},{"$f":"'Schedule 17'!H488","v":{"v":735000,"d":"735,000.00"}}]
[]
[null,null,"18","SCHEDULE 18 - CHEMICAL BUILDING",{"$nulls":3},{"$f":"'Schedule 18'!H383","v":{"v":185000,"d":"185,000.00"}}]
[]
[null,null,"19","SCHEDULE 19 - COMMISSIONING & DOCUMENTATION",{"$nulls":3},{"$f":"'Schedule 19'!H146","v":{"v":0,"d":"0.00"}}]
{"$rows_empty":21}
[null,null," Total"," Total",{"$nulls":3},{"$f":"SUM(H3:H60)","v":{"v":12463145,"d":"12,463,145.00"}}]

{"sheet":"Rate Estimator","index":20,"n_rows":17,"n_cols":3,"rows_kept":17}
[]
[null,null,"To use a free rate estimator program with this Excel file"]
[]
[null,"1)","Download and install the program by clicking the link below and following instructions"]
[null,null,"Bill Project (demo mode)"]
[null,"2)","In MS Windows run the program using 'Start > Programs > Civilsoft > Bill Project'"]
[null,"3)","Once Bill Project is running use 'File > Open Excel Tender' and select this file, eg"]
[null,null,{"$f":"MID(CELL(\"filename\"),1,FIND(\"]\",CELL(\"filename\")))","v":"C:\\Users\\DeveshR\\Documents\\Bill Project\\Printouts\\[WS7382_BOQ 20250527.xlsx]"}]
[null,"4)","Item rates can now be calculated by adding project resources to items"]
[null,"5)","For more information in Bill Project use 'Tools > Guide' and click on 'Rate Estimator'"]
[]
[null,null,"Note:"]
[null,null,"Although Bill Project will be set to demo mode, the rate estimator will have full functionality"]
[null,null,"Once rates have been calculated in Bill Project they can be exported using 'File > Export > Rate'"]
[]
[null,null,"If you need help with any of the above, click the link below or phone +27 (0)42 294 1777"]
[null,null,"Bill Project support"]