{"text_format":"3","workbook":"xls","n_sheets":13,"sheets":["Cover","PREAMBLE ","SCHEDULE A - P & G","SCHEDULE B - ENVIRONMENTAL","SCHEDULE C - SHEQ","SCHEDULE D - QUALITY","SCHEDULE E - Automation","SCHEDULE F - CIVIL","SCHEDULE G - ELECTRICAL","SCHEDULE H - Mechanical","SCHEDULE I - PIPELINE","SCHEDULE J - SED","Summary"],"not_rendered":{"images":11,"external_links":2,"defined_names":13},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Cover","index":0,"n_rows":21,"n_cols":4,"rows_kept":21,"merged":[[1,7,2,7],[6,1,7,1],[18,2,18,5]],"flags":["formulas_cached_only"]}
{"$rows_empty":11}
[{"$nulls":3},"BILL OF QUANTITIES"]
[]
[]
["DATE:",null,null,"NOVEMBER 2021"]
[]
[]
["PROJECT TITLE:"]
[null,null,"VEREENIGING PUMPING STATION - CATHEDRAL HEADER"]
[]
["SAP PROJECT NUMBER:",null,null,"P.03341"]

{"sheet":"PREAMBLE ","index":1,"n_rows":166,"n_cols":2,"rows_kept":166,"merged":[[40,0,40,1],[41,0,41,1],[82,0,82,1],[83,0,83,1],[128,0,128,1],[129,0,129,1]],"flags":["formulas_cached_only"]}
[null,"Preamble and Pricing Instructions"]
[1,"Definition of The Scope of Scheduled Items"]
[1.1,"Preamble and Pricing Instructions"]
["1.1.1","The prices and rates to be inserted in Bills of Quantities are to be the fully inclusive prices for the work described under the Price Schedules therein. Such prices and rates shall cover all costs and expenses that may be required in and for the execution of the work described, and shall cover the cost of all general risks, liabilities, and obligations set forth or implied in the documents on which the tender is based, as well as overhead charges and profit. This shall include any documentation or attendance of mandatory safety induction. Reasonable prices shall be inserted, as these will be used as a basis for assessment of payment for additional work that may have to be carried out."]
[]
["1.1.2","A price or rate is to be entered against each item in Bills of Quantities, whether the quantities are stated or not. Items that are required to be inserted in the Provisional Bills of Quantities by the Contractor, and which have not been duly inserted, shall be considered as covered by other rates or prices in the Provisional Bills of Quantities."]
[]
["1.1.3","Except where rates only are required, insert all amounts to be included in the total tendered price in the \"Amount\" column and show the corresponding total tendered price."]
[]
["1.1.4","The units of measurement described in the Bills of Quantities are in metric units."]
[]
["1.1.5","The Price Schedule is provisional and shall be subject to finalisation of the requirements on site and accurate measurement of actual quantities installed on site by the Contractor. The Contractor shall verify all quantities, dimensions, etc by actual measurement on site before the ordering of material, etc.  Rand Water does not accept responsibility for under or over measure as a result of the failure of the Contractor to verify quantities and dimensions before ordering. Jointing of e g cables which have resulted due to erroneous measurements will not be accepted."]
[]
["1.1.6","The quantities in the Provisional Schedules are estimates of the final quantities to enable the Contractor to determine the magnitude and scope of the works.  Payment will be made on final measurement of quantities of each item of the work on site."]
[]
["1.1.7","The Contractor in executing the work or in ordering any Contractors equipment or in ordering any plant shall not be guided by or work to any descriptions, dimensions or quantities as set forth in the Provisional Bills of Quantities.  He/she shall be guided by and work to the drawings supplied for the works, specifications and by the instructions of the Engineer and measurements taken on site."]
[]
["1.1.8","Where Provisional Sums appear in the Bills of Quantities the contractor shall provide competitive quotations with breakdowns of costs for work required and agreed, and payments will be against these quotations taking into account the contractors mark up. All items described as \"Provisional\" shall be measured as executed and paid for according to prices in the Bills of Quantities and any unexpended amounts shall be deducted from the amount of the Contract Sum.  No work for which \"Provisional\" items are provided shall be commenced without written instructions from the Engineer."]
[]
["1.1.9","System Specification Clause column is provided to make it easier for the Contractor to quickly locate some of the major clauses pertaining to that equipment/works within the System Specifications document. It is still the responsibility of the Contractor to thoroughly read through the entire System Specification document (including the entire Tender Documents, Drawings, Applicable Standards and Site Information) identify other applicable clauses pertaining to an equipment/works that have not been stated in the System Specification Clause column."]
[]
["1.1.10","These Bills of Quantities shall be used to assist both parties in administering and agreeing any changes/variations, which may arise during the course of the Contract."]
[]
["1.1.11","These Bills of Quantities shall be used to calculate the value of work completed in the evaluation of interim/final payments."]
[]
["1.1.12","The Contractor is deemed to have allowed opposite each item contained in these Bills of Quantities whatever costs and charges it may consider necessary for the carrying out, complying with and due observance of the provisions, conditions and requirements set out in the Contract."]
[]
["1.1.13","No claim whatsoever will be entertained in respect of errors or omissions in pricing due to the brevity of a description of any item contained in these Bills of Quantities which items are fully described or can reasonably inferred when read in conjunction with the relevant clauses provided for in the Conditions of Contract, Specifications, Drawings or other relevant documentation.  "]
[]
["1.1.14","Any item left un-priced will be deemed to be provided for elsewhere and no claim for any extras arising out of the Contractor’s omission to price any item will be entertained."]
["1.1.15","Whatever rate the tenderer puts in the Bill of Quantities as “rate only” shall be subject to verification by Rand Water quantity surveyors during project implementation."]
[]
["1.1.16","For the purposes of this schedule of quantities, the following words shall have the meaning hereby assigned to them:"]
[]
[null,"·         Unit: The unit of measurement for each item of work as defined in the specifications."]
[]
[null,"·         Quantity: The number of units of work for each item."]
[]
[null,"·         Rate: The payment per unit of work for which the tenderer tenders to do the work."]
[]
[]
[]
[null,"·         Amount: An amount tendered for an item, the extent of which is described in the schedule of quantities, the specification or elsewhere, but of which the quantity of work is not measured in units."]
[]
["1.1.17","The Form of Tender, the General and Particular Conditions of Contract, the Specification            and Drawings shall be read in conjunction with the price schedule."]
[]
["1.1.18","The price schedules and summary of price schedules shall be priced, extended, totalled and signed by the Tenderer. The total tender price shall be carried to the Form of Tender.  The Form of Tender and the Schedules shall be completed and signed."]
[]
["1.1.19","The tender price will be taken to be the price entered in the Form of Tender.  In the event of discrepancies between tendered rates and extended amounts in the price schedule, the amounts will be deemed to be correct and the rates will be corrected accordingly.  In the event of discrepancies between extended amounts and the total tender price entered in the Form of Tender, the total tender price will be deemed to be correct and adjustments made by agreement to rates and extended amounts."]
[]
["1.1.20","The quantities set out in the Schedule of Quantities are the estimated quantities of the Contract Works, but the Contractor will be required to undertake whatever quantities may be directed by the Engineer from time to time.  The Contract Price for the completed contract shall be computed from the actual quantities of work done, valued at the relevant unit rates and prices. The validity of the contract shall in no way be affected by differences between the quantities in the schedule of quantities and the quantities finally certified for payment.  Work shall be valued at the rates or lump sums tendered, subject only to the provisions of the general conditions of contract."]
[]
["1.1.21","All rates and sums of money quoted in the schedule of quantities shall be in Rands and whole cents.  Fractions of a cent shall be discarded."]
["1.1.22","The Employer shall without prejudice retain the rights to exclude and/or include certain aspects of the Bill of Quantities"]
[]
["1.1.23","The items included in Bills of Quantities are a guideline to the contractor.  It is the Contractor’s responsibility to thoroughly familiarise himself with all of the works information and specifications for this Contact so as to ascertain the scope and extent of the works and ensure that any items that are required to achieve the functional requirements of this Contract are included in the Bill of Quantities."]
[]
["1.1.24","Where no requirement has been stated in the documentation for Technical Data Sheets, Tenderers shall provide for items as reflected in the “measurement and payment” clauses of the applicable standard specification (e.g. SABS 1200 series specifications)."]
[]
["1.1.25","The description of each item shall, unless otherwise stated herein, be held to include making, conveying and delivering, unloading, storing, unpacking, hoisting, setting, fitting and fixing in position, cutting and waste, patterns, models and templates, plant, temporary works, return of packings, establishment charges, profit and all other obligations arising out of the Conditions of Contract."]
[]
["1.1.26","Unless a separate rate for the supply and for the installation of any item is specifically called for, the supply, delivery and installation costs of any item shall be fully included in the unit price."]
[]
["1.1.27","No alteration, erasure or addition is to be made in the typed text of the Bills of Quantities.  Should any alteration, erasure or addition be made other than in the areas allowed for this, it will not be recognised but the original wording of the Bill of Quantities will be adhered to."]
[]
["1.1.28","The Tenderer shall not be relieved of responsibility for measuring quantities at the Tender stage, and the Tender Sum submitted shall be in respect of the quantities set out in the Bills of Quantities.  The Tenderer shall be required to make his assessment and allowance of sundry equipment such as gaskets, bolts, nuts, brackets, fixing, etc., to form part of his pricing and shall include in the item prices for such small installation materials as are required for complete installation in accordance with the Specification."]
[]
["1.1.29","The following abbreviations are used in the schedule of quantities:"]
[null,"mm = millimetre"]
[null,"m = metre"]
[null,"m² = square metre"]
[null,"m³ = cubic metre"]
[null,"t = tons"]
[null,"No = number"]
[null,"PC Sum = prime cost sum"]
[null,"Prov Sum = provisional sum"]
[2,"Electrical Preamble"]
[2.1,"Design and detailing of the installation"]
[null,"Items are provided in the Provisional Bills of Quantities for final design suitable for construction of the Substation Distribution Board and the Mimic Panel. Included is marking up Rand Water’s schematic diagrams, general arrangement layout, door layouts, selection of equipment and planning the chassis layouts with wiring channels, labels, terminals etc."]
[null,"The final planning of cable routes, detailed cable racking layouts and design considering cable runs to minimise cross overs, mechanical strength of the racking system wherever required is included. Also included is detailed liaison with Eskom with respect to cable runs in their switchyard."]
[null,"The contractor shall also determine the best positions for installation of the Distribution Board, Mimic Panel and UPS, and core drilling into the Engine Room basements where required for cable access."]
[2.2,"Documentation"]
[]
[]
[null,"The contractor shall provide as built drawings in latest version Autocad format of all distribution boards inclusive of dimensioned general arrangements, schematic diagrams, labels etc."]
[null,"Detailed as installed cable schedules and earthing conductors with installed lengths of cable shall be provided in electronic and hard copy format."]
[null,"Marked up dimensioned cable route drawings shall be provided for updating by Rand Water."]
[null,"Certification inclusive of test certificates, FAT certificates, assembly assessors certificate and Certificates of Compliance shall be provided in hard copy and electronic formats."]
[2.3,"Supply and delivery of cables"]
[null,"In determining the length of cable installed the gland to gland distance will be measured plus additional cable per end as determined below:"]
[null,"a) End at 400 V and 11kV switchgear - 1,5 metres"]
[null,"b) End at any other device - 0,5 metre"]
[null,"Separate items will be scheduled for each type, size and number of cores of cables supplied and/or installed.  The rates shall apply for installation of cables at all levels.  Should cable be required to be installed at levels above two metres completed working platforms (and ground level) an additional rate will be applied reflecting actual costs for scaffolding, scaffold planks, boarding, labour to erect scaffolding etc."]
[]
[2.4,"Cables - supply and install"]
[null,"a) Rates shall include full compensation for the procurement, delivery to site, unloading and on site storage, protection, handling, craneage, measurement of cable runs, cutting, installing the cable in accordance with the specification (including cable jacks and rollers) laying in cable ducts or on cable racking complete with identification tagging and labelling.  Rates shall also include the supply and fixing of all clamps, trefoil clamps for single core cables, cable straps or cable ties etc.  The testing of Medium Voltage cables will be by the Overvoltage Low Frequency Method and by On Line Partial Discharge three months after commissioning. The testing of all 600/1 000 V PVC, PVC, SWA, PVC cable with 1 000 V DC megger shall also be included in the rates.  Instrumentation signal cables shall not be tested with a megger."]
[]
[null,"b) All power and control cables supplied shall comply with SABS 1507 and 1339 Type A and B where applicable and shall bear the SABS mark. Cables shall be 6.35/11 kV XLPE and 600/1 000V PVC, PVC, SWA, PVC with copper conductors and flame retardant, outer sheaths.  "]
[2.5,"Cables - installation only"]
[null,"The rates for the installation only of cables shall include full compensation for the unloading and on site storage, protection, handling, cranage, measurement of cable runs, cutting, installing the cable in accordance with the specification (including cable jacks and rollers) fixing the cable to cable racking with cable ties, complete with identification tagging and labelling. "]
[2.6,"Cable termination"]
[null,"A termination rate is defined as one cable end.  Separate rates shall be supplied for each type of cable end.  Rates shall include full compensation for the supply of all cable glands, tapes, shrouds, termination kits, cutting, stripping, lacing/harnessing crimping, lugs and cable core numbering ferrules in accordance with the specification. The drilling of gland plates shall also be included in rates as well as the treatment of metal parts with cold galvanising paint "]
[2.7,"Cable trenches - excavation and backfill"]
[null,"The excavation and backfilling of cable trenches shall be measured on a cubic meter basis."]
[]
[null,"Rates shall include full compensation for the setting out, supervision, labour, materials, provision of all necessary equipment to complete the backfilling process including the cleaning out of trenches, supply and laying sieved stone free soil or sand, supply, backfilling and compaction of trenches in accordance with the specifications."]
[]
[null,"The rates shall include for the barricading of open cable trenches with orange netting type barricade (danger tape not acceptable)."]
[]
[null,"The contractor shall also protect open cable trenches against subsidence and filling with storm water."]
[]
[null,"The contractor shall repair the tar roads after installation of sleeves as per the Rand Water specification."]
[]
[null,"The contractor shall also measure on a per meter basis for the supply and installation of concrete paving slabs and danger tape in all cable trenches."]
[]
[null,"The excavation of trenches is defined in the terms of the specification as Class 1 soft pickable material or Class 2 Hard Rock. Unless otherwise stated all excavation shall be carried out by hand."]
[]
[null,"Excavations will be classified in two categories only."]
[]
[null,"a) Class 1: Pickable, Earth, hand pickable and soft rock. All ground types including hand pickable rock which do not have to be removed by pneumatic drill, blasting, wedging or other mechanical means. The material may contain significant proportions of boulders and rock which can be removed manually."]
[]
[null,"b) Class 2: Hard Rock, All ground types which can only be broken by pneumatic drill, wedging or other mechanical means."]
[]
[null,"Excavations are measured in the Bills as Class 1 (Pickable) and Class 2 (Hard Rock). No excavations shall be deemed to be Hard Rock unless certified by the Engineer. The Engineer shall be called to site by the Contractor to inspect and certify occurrence of Hard Rock."]
[]
[null,"Cable markers will be measured separately and measured by number. Rates for cable markers shall include full compensation of the manufacture, delivery to site, handling, storage and installation on completion of cable trenching."]
[]
[2.8,"Cable racking - supply and install"]
[]
[]
[null,"Cable racking will be measured by length as installed between fittings which will be measured by number. Separate items are scheduled for each type and size of cable rack, cable rack fittings such as 90 degree bends, tees, elbows, reducers etc for each type and size of rack."]
[]
[null,"Rates shall include full compensation for supply, delivery, storage, installation, cutting, application of corrosion protection, splices, nuts and bolts, drilling, support brackets including spring nuts and bolts, steelwork, tools and hilti/rawl bolts necessary to complete the installation."]
[]
[null,"Where cable racks are installed in the horizontal plane, racks shall be supported at a minimum of 1,2 metre intervals. Where cable racks are installed in the vertical plane, racking shall be supported at a minimum of 1, 5 metre intervals. The support brackets, unistrut supports, painting and treatment of steelwork are inclusive in the cable racking and rates are to be calculated on this basis."]
[]
[null,"The earthing of cable racks shall be measured as a separate item."]
[2.9,"Cable joints - supply and install"]
[null,"Cable joints will be measured by number.  Separate items will be scheduled for each type of kit and cable to be joined."]
[]
[null,"Rates shall cover full compensation for the jointing kits, all labour including specialist labour as required, ferrules, crimping, tape, materials, tools and necessary protection covers for outdoors whilst jointing."]
[]
[2.1,"Earthing and Suppression - supply and install"]
[null,"The Contractor shall connect each plant item e.g. 11kV switchboard and distribution board, etc to the applicable station earth bar.  No allowance will be made for slack, at joints or connections to equipment etc. Earthing will be measured from lug to lug and separate items will be scheduled for copper coated steel wire or insulated earth wire for each size of conductor run with individual circuits.  Rates shall include full compensation for installing the earthing including supply, delivery, measuring of runs, installing in terms of the specification and strapping and supporting as necessary."]
[]
[2.11,"Miscellaneous equipment - supply and installation"]
[null,"The supply and installation of miscellaneous items such as statutory labels, equipment labels and any other piece of equipment not covered in previous clauses will be measured by number  where possible, alternatively by a sum amount."]
[]
[null,"Rates shall include full compensation for the supply, delivery to site, storage, transport, labour handling, brackets, bolts, corrosive protection and fixings."]
[]
[2.12,"Testing and Commissioning"]
[null,"Separate items will be scheduled for the testing and commissioning of MV and LV switchgear, UPS, Mimic Panel and all power cables. Test equipment to be supplied for commissioning shall include but be limited to the following and shall be available on site at all times:"]
[]
[null,"Two off portable electronic instruments (Fluke or approved equivalent)"]
[null,"Two off clip on tong testers (Robin mod 2006F, Fluke or approved equivalent)"]
[null,"500 V / 1 000 V megger"]
[]
[3,"Architecture Preamble"]
[]
[null,"Refer to Standard System of Measuring Building Work 7th Ed: ISBN: 978-0-86886-837-0; The Asscociation of South African Quantity Surveyors"]
[]
[4,"Civil and Pipeline Preamble"]
[]
[4.1,"All tenderers are to ensure that they familiarise themselves with the variations and additions to SANS 1200 which are provided as part of the contract documentation."]
[]
[4.2,"The Tenderer shall state separately against each item the rate per metre of pipe that shall be deemed to include the full inclusive cost of providing the material and of carrying out the work required to manufacture the steel pipe shell, provide the coatings and for the transport to the route of the pipelines, all in accordance with Sub- Clause 7.1 of the Conditions of Contract Fidic Redbook.  The rate shall include all conditions, liabilities, general risks and obligations set forth or implied in the Contract Documents. The preamble hereafter headed Methods of Measurement and Payment regarding the scope of the prices and rates shall be taken as amplifying but not limiting Sub-Clause 7.1 of the Conditions of Contract Fidic Redbook."]

{"sheet":"SCHEDULE A - P & G","index":2,"n_rows":139,"n_cols":7,"rows_kept":139,"merged":[[0,2,0,5],[1,2,1,4],[1,7,2,7],[6,1,7,1],[57,0,57,4],[58,0,58,4],[103,0,103,4],[104,0,104,4],[132,2,132,5],[133,2,133,5],[134,2,134,5],[135,2,135,5],[136,2,136,5],[137,2,137,5],[138,1,138,5]],"flags":["formulas_cached_only"]}
[null,null,"CONSTRUCTION OF THE CATHEDRAL HEADER CHAMBER AT"]
[null,null,"VEREENIGING PUMPING STATION",{"$nulls":3},"Preliminary and General"]
[]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No.","Refers"]
[]
["A","SABS 1200A","PRELIMINARY & GENERAL "]
[]
["A1",null,"FIXED CHARGED ITEMS"]
[]
["A1.1","8.3.1","Contractual requirements","SUM",1]
[]
[null,null,"ESTABLISH FACILITIES ON THE SITE FACILITIES FOR THE ENGINEER (SANS 1200AB)"]
[]
["A1.2","8.3.2.1","Engineer's offices and facilities","SUM",1]
[]
["A1.3","8.4.2.1 (d)","Survey Instruments","SUM",1]
[]
[null,null,"SERVICES"]
[]
["A1.4","8.3.2.2","Services for offices and for cooking and ablution facilities on site for the Engineer's site staff","SUM",1]
[]
["A1.5",null,"Treatment and maintenance of areas surrounding offices","SUM",1]
[]
["A1.6","8.3.2.1(c )","Name board (including posts and erection)","No",1]
[]
["A1.7",null,"SANS 1200 Standardized Specifications","SUM",1]
[]
[null,null,"FACILITIES FOR CONTRACTOR"]
[]
["A1.8","8.3.2.2 (a)","Offices and storage sheds","SUM",1]
[]
["A1.9","8.3.2.2 (b)","Workshops","SUM",1]
[]
["A1.10","8.3.2.2 (d)","Living accommodation","SUM",0]
[]
["A1.11","8.3.2.2 (e)","Ablution and latrine facilities","SUM",1]
[]
["A1.12","8.3.2.2 (f)","Tools and equipment","SUM",1]
[]
["A1.13","8.3.2.2 (g)","Water supply, electric power, communications, dealing with water and access","SUM",1]
[]
["A1.14","8.3.4","Removal of Engineer's and Contractor's site establishment on completion","SUM",1]
[]
["A2",null,"TIME RELATED ITEMS"]
[]
["A2.1","8.4.1","Contractual requirements","Month",24]
[]
["A2.2","8.4.1","Surety or bank guarantee","Month",24]
[]
["A2.3","8.4.1","Third party insurance","Month",24]
[]
["A2.4","8.4.1","Insurance of construction plant and equipment","Month",24]
[]
["A2.5","8.4.1","Other (detail………………………………………………………)","Month",24]
[]
[]
["TOTAL CARRIED FORWARD ",{"$nulls":4},"R"]
["TOTAL BROUGHT FORWARD ",{"$nulls":4},"R"]
[]
[null,null,"OPERATE AND MAINTAIN FACILITIES ON THE SITE FOR ENGINEER FOR THE DURATION OF CONSTRUCTION"]
[]
["A2.6","8.4.2.1 (a)","Engineer's offices and facilities","Month",24]
[]
["A2.7","8.4.2.1 (d)","Survey Instruments","Month",24]
[]
[null,null,"SERVICES"]
[]
["A2.8","8.4.2.1 (a)","Services for offices and for cooking and facilities on site for the Engineer's staff","Month",24]
[]
["A2.9","8.4.2.1 (d)","Survey assistants","Month",24]
[]
["A2.10",null,"Treatment and maintenance of areas surrounding offices ","Month",24]
[]
["A2.11","8.4.2.1 (c)","Name board","Month",24]
[]
[null,null,"FACILITIES FOR CONTRACTOR FOR THE DURATION OF CONSTRUCTION"]
[]
["A2.12","8.4.2.2 (a)","Offices and storage sheds","Month",24]
[]
["A2.13","8.4.2.2 (b)","Workshops","Month",24]
[]
["A2.14","8.4.2.2 (d)","Living accommodation","Month",24]
[]
["A2.15","8.4.2.2 (e)","Ablution and latrine facilities","Month",24]
[]
["A2.16","8.4.2.2 (f)","Tools and equipment","Month",24]
[]
["A2.17","8.4.2.2 (g)","Water supply, electric power, communications, dealing with water and access","Month",24]
[]
["A2.18","8.4.3","Supervision","Month",24]
[]
["A2.19","8.4.4","Company and head office overhead costs","Month",24]
[]
["A2.20","8.4.5","Testing and commissioning of equipment","Month",24]
[]
["A3",null,"PROVISIONAL SUMS"]
[]
["A3.1",null,"Geotechnical investigations","Prov. Sum",1,{"v":300000,"d":"300,000.00"},{"v":300000,"d":"300,000.00"}]
[]
["A3.2",null,"Contractors mark-up on item A3.1 aove","%",{"v":300000,"d":"300,000.00"}]
[]
[]
["TOTAL CARRIED FORWARD ",{"$nulls":4},"R"]
["TOTAL BROUGHT FORWARD ",{"$nulls":4},"R"]
[]
["A4",null,"TEMPORARY WORKS"]
[]
[null,null,"EXISTING SERVICES"]
[]
["A4.1","8.8.4","Excavate by hand to expose existing services (provisional)","m2",100]
[]
["A4.2","8.8.4","Protection of existing services","SUM",1]
[]
[null,null,"SURVEY AND REFERENCE PEGS"]
[]
["A4.3","8.8.5","Protect and re-establish all reference pegs and bench marks","SUM",1]
[]
[null,null,"PUBLIC LIAISON OFFICER (Provisional Item)"]
[]
["A4.4",null,"Remuneration of public liaison officer for the duration of the contract","Item","1.00"]
[]
["A4.5",null,"Contractor's charges to provisional amount above","%","15.00"]
[]
[null,null,"ITEMS NOT MENTIONED"]
[]
["A4.6",null,"Should the Contractor wish to price any items mentioned in the General Conditions of Contract, Specifications or Drawings but not specifically mentioned in the Schedule, he should do so hereunder. Full descriptions, quantities, units and rates are to be stated.","Item","1.00"]
[]
["A4.7",null,"Site visits for assessment of equipment","SUM",1]
[]
["A4.8",null,"Compiling of documentation","SUM",1]
[]
[null,null,"Total amount excluding Value-Added Tax (VAT) to be carried to Summary of Price Schedules "]
["No","Payment refers","Description",{"$nulls":3},"Amount"]
[]
[]
[]
[]
[null,"Total amount excluding Value-Added Tax (VAT) to be carried to Summary of Price Schedules "]

{"sheet":"SCHEDULE B - ENVIRONMENTAL","index":3,"n_rows":63,"n_cols":7,"rows_kept":63,"merged":[[0,2,0,5],[1,0,2,1],[1,2,1,4],[12,0,16,0],[12,3,16,3],[12,4,16,4],[21,3,27,3],[21,4,27,4],[28,0,31,0],[28,3,30,3],[28,4,30,4],[36,0,36,4],[37,0,37,4],[56,0,56,6],[57,2,57,5],[58,2,58,5],[59,2,59,5],[60,2,60,5],[61,2,61,5],[62,1,62,5]],"flags":["formulas_cached_only"]}
[null,null,"CONSTRUCTION OF THE CATHEDRAL HEADER CHAMBER AT"]
[null,null,"VEREENIGING PUMPING STATION"]
[]
[{"$nulls":6},"SCHEDULE B: ENVIRONMENT"]
[]
["Item ","Payment","Description","Unit","Qty","Rate","Amount"]
["No.","Refers"]
[null,null,"SCHEDULE B:  ENVIRONMENT"]
["B","PSA 8.3.14","ENVIRONMENT"]
["B1",9.1,"Administrative requirements as per environmental specification.                                             • Understanding of compliance\n• Preparation of environmental file and work program approval.\n• Preparations of method statements (management of all waste, Keeping the site clean and weed free, final clean up of site and campsite). \n• Maintaining of auditing of site compliances\n• Reporting of environmental incidence\n• Signing off of work for payment \n• Emergency preparedness retainement for external services\n• Programme scheduling details of administrative matters:\n","Sum",1]
[]
[null,9.2,"Emergency preparedness funding"]
["B2",null,"a)          Provision for bee, snake and other fauna removal","Sum",1]
[null,null,"b)          Provision for hydrocarbon spillages that require intervention from professional clean up provider"]
[null,null,"c)           Provision to clean up sewage spillages"]
[null,null,"d)          Equipment for fire fighting"]
[null,null,"e)          Call out of fire department"]
["B3","9.1.4","Environmental awareness and training "]
[null,null,"The rate for this item shall include costs for inductions and environmental awareness and training","Sum",1]
["B4",9.2,"Social integration of the project to the public "]
[null,null,"The rate for this item shall include costs for establishment of construction campsite and working areas","Sum",1]
["B5",9.3,"Establishment of site camp and works area.","Sum",1]
[null,null," "]
[null,null,"·        The contractor’s contact numbers"]
[null,null,"·        ECO details "]
[null,null,"·        Emergency numbers and provision for: – snake removal, bee removal, fire, large hydrocarbon spillages, sewerage spillages"]
[null,null,"Signage measuring a minimum of 30mmx30mm must also be made available for no go areas."]
["B6","9.3.4 to 9.3.4.2","Barricading and demarcation"]
[null,null,"a.      Screening for unsightly works","sum",1]
[null,null,"b.     Clear demarcating of the working foot print"]
[null,null,"c.      Barricading of sensitive no go areas"]
[]
["B7","9.4 to 9.4.6","Pollution prevention and preservation of environmental resources "]
["B8",null,"The rate for this item shall include costs for  pollution prevention and preservation of environmental resources","sum",1]
["B9",null,"a) Cleaning the site of litter and rubble","sum",1]
[]
["TOTAL CARRIED FORWARD ",{"$nulls":4},"R"]
["TOTAL BROUGHT FORWARD ",{"$nulls":4},"R"]
[]
["B10",null,"b)Weed control on site","sum",1]
["B11",null,"C)          Waste bins and receptacles that comply with the waste clauses of the Environmental specification.","sum",1]
["B12",null,"c)  Appropriate skips for waste separation","sum",1]
["B13",null,"d)General waste Waste removal","sum",1]
["B14",null,"e)Hazardous waste Waste removal","sum",1]
["B15",null,"f)Recycled waste management  Waste removal","sum",1]
["B16",null,"g) Spillage kits to clean up spillages  ","sum",1]
["B17",null,"h) Hard impervious surfaces for storage of chemicals","sum",1]
["B18",null,"i)Bunding facility for hazardous products","sum",1]
["B19",null,"J)          Labelled containers for decanting of liquids","sum",1]
["B20",null,"K) Drip trays for all vehicles staying on site over night","sum",1]
[null,9.5,"Preservation of the environment: fauna ,flora, scenic value,  Archaeological artefacts"]
["B21","9.5.3","Erosion control and silt management The amount shall represent the costs associated with the practice of preventing or controlling wind or water erosion during construction. The erosion control measures must effectively prevent water pollution, soil loss, wildlife habitat loss and human property loss.  The rate shall also include the costs of silt control where devices shall be designed to keep eroded soil on a construction site, so that it does not wash off and cause water pollution to a nearby stream, river, lake, or dam.","Lump Sum",1]
["B22",null,"Final clean up and rehabilitation of the construction camp to the state in which it was prior to comencement of work","Lump Sum",1]
["B23",null,"Appointment of an environmental officer","sum",1]
[]
[]
["ENVIRONMENTALSUMMARY "]
["No","Payment refers","Description",{"$nulls":3},"Amount"]
[]
[]
[]
[]
[null,"Total amount excluding Value-Added Tax (VAT) to be carried to Summary of Price Schedules "]

{"sheet":"SCHEDULE C - SHEQ","index":4,"n_rows":65,"n_cols":7,"rows_kept":65,"merged":[[0,2,0,5],[1,0,2,1],[1,2,1,4],[4,0,5,0],[4,1,5,1],[4,5,5,5],[38,0,38,4],[39,0,39,4],[52,3,52,5],[58,0,58,6],[59,2,59,5],[60,2,60,5],[61,2,61,5],[62,2,62,5],[63,2,63,5],[64,1,64,5]],"flags":["formulas_cached_only"]}
[null,null,"CONSTRUCTION OF THE CATHEDRAL HEADER CHAMBER AT"]
[null,null,"VEREENIGING PUMPING STATION"]
[]
[{"$nulls":6},"Schedule C: SHEQ"]
["Item   No.","Payment Refers","Description","Unit","Qty","Rate","Total Amount"]
[]
[]
[null,null,"Please refer to Preamble document"]
["C",null,"HEALTH AND SAFETY"]
["C1.1","2.4 & 2.5.","Preparation of the Contractor's site specific Health and Safety Plan","lump sum",1]
[]
["C1.2",3.2,"Principal Contractor's initial obligations in respect of the Occupational Health and Safety Act and Construction Regulations","lump sum",1]
[]
["C1.3",4,"Principal Contractor's time related obligations in respect of the Occupational Health and Safety Act and Construction Regulations","Month",24]
[]
["C1.4","10.d","Provision of Personal Protective Equipment (PPE)","lump sum",1]
[]
["C1.5","3.2.1","Provision of a full-time Construction Health and Safety Officer","Month",24]
[]
["C1.6",15,"Cost of medical certificates and medical surveillance"]
[]
[null,15,"(a) Initial (baseline) medical examinations","lump sum",1]
[]
[null,15,"(b) Periodic  examinations","lump sum",1]
[]
[null,15,"(c)Exit examinations","lump sum",1]
[]
["C1.7",9.3,"Induction training","lump sum",1]
[]
["C1.8",16,"Provision of First Aid Boxes to GSR requirements and other emergency safety equipment such as fire extinguishers.","lump sum",1]
[]
["C1.9","24 C09","Transportation of Workers","lump sum",1]
[]
["C1.10",11,"Welfare Facilities","lump sum",1]
[]
["C1.11",14,"Occupational Hygiene Surveys","lump sum",1]
[]
["C1.12",10,"Training","lump sum",1]
["TOTAL CARRIED FORWARD ",{"$nulls":4},"R"]
["TOTAL BROUGHT FORWARD ",{"$nulls":4},"R"]
["C1.13","Part B (Annexure 11.1)","Security requirements including the security risk assessment (before site establishment)","lump sum",1]
[]
["C1.14","24 C14, 7 ","Employee wellness programs","lump sum",1]
[]
["C1.15",7,"Drug and Alcohol Testing, Policies and Procedures","lump sum",1]
[]
["C1.16","Part B 10 k","Barricading","lump sum",1]
[]
["C1.17","Part B 10 a ","Safety notices and signs","lump sum",1]
[]
["C1.18",8,"SHE  Incentives","lump sum",1]
[]
["C1.19","3.2.1 & 5C","COVID-19 Prevention and Management: The Engineer to advise at the relevant stage after award","PC SUM"]
[]
["C1.20","Part B 10n,6.6 ","Adequate ventilation and lighting during construction","lump sum",1]
[]
["C1.21",2.9,"Submission of the Health and Safety File (hard and soft copies)","lump sum",1]
[]
["SHEQ SUMMARY "]
["No","Payment refers","Description",{"$nulls":3},"Amount"]
[]
[]
[]
[]
[null,"Total amount excluding VAT to be carried to Summary of Price Schedules "]

{"sheet":"SCHEDULE D - QUALITY","index":5,"n_rows":41,"n_cols":7,"rows_kept":41,"merged":[[0,2,0,5],[1,0,2,1],[1,2,1,4],[5,1,6,6],[8,0,9,0],[8,1,9,1],[8,5,9,5],[12,1,13,1],[35,0,35,6],[36,2,36,5],[37,2,37,5],[38,2,38,5],[39,2,39,5],[40,1,40,5]],"flags":["formulas_cached_only"]}
[null,null,"CONSTRUCTION OF THE CATHEDRAL HEADER CHAMBER AT"]
[null,null,"VEREENIGING PUMPING STATION"]
[]
[{"$nulls":6},"SCHEDULE D: QUALITY"]
[]
[null,"OVERFLOW PIPE DIVERSION, AUTOMATION AND ELECTRICAL UPGRADES AT MEYERSDAL RESERVOIR"]
[]
[{"$nulls":6},"Schedule D: Quality"]
["Item   No.","Payment Refers","Description","Unit","Qty","Rate","Total Amount"]
[]
[]
[null,null,"Please refer to Preamble document"]
["D","SAM QA 00030 Pr clauses"]
[]
["D1",7.1,"Preparation and submission of Contractors Quality Management Plan (CQMP), for review and approval prior to commencement of works","  Sum",1]
[]
["D2","7.5.3","Provision of Qualified Quality Officer ( The contractor shall provide RW with relevant to the scope of work  qualified Quality Officer )","Rate ",1]
[]
["D3",7.4,"Maintenance of documents and final documentation for submission ","Sum "]
[]
["D4","7.5.5","Provision of Quality Officers relevant training ( The contractor to provide related training for the quality officer ) ","Rate ",1]
[]
["D5","7.6.2","Provision of Compliance Audits ( The contractor to audit the project once a year for the duration of the project ) ","Rate ",1]
[]
["D6","7.5.4","Testing Equipment calibration ( The testing Equipments should be calibrated as per the manual ) ","Rate ",1]
[]
["D7","7.6.2","Welders qualification  training as per the code ( The contractors must qualify the welders as per API 5L ) ","Rate ",1]
[]
["D8","7.6.1","Provision of any other  testing and inspections requested by the Engineer","Sum ",1]
[]
["D9",null,"The contractor to perform the Non Destructive Services to welded structure as per the Specification "]
["D9.1",null,"Xray ","Rate ",1]
["D9.2",null,"MPT","Rate ",1]
["D9.3",null,"PT","Rate ",1]
[]
["QUALITY SUMMARY "]
["No","Payment refers","Description",{"$nulls":3},"Amount"]
[]
[]
[]
[null,"Total amount excluding Value-Added Tax (VAT) to be carried to Summary of Price Schedules "]

{"sheet":"SCHEDULE E - Automation","index":6,"n_rows":96,"n_cols":7,"rows_kept":96,"merged":[[0,2,0,5],[1,2,1,4],[1,9,1,11],[2,9,2,11],[4,1,5,1],[95,0,95,2]],"flags":["formulas_cached_only"]}
[null,null,"CONSTRUCTION OF THE CATHEDRAL HEADER CHAMBER AT"]
[null,null,"VEREENIGING PUMPING STATION",{"$nulls":3},"SCHEDULE F: AUTOMATION"]
[]
[]
["Item No","Payment Refers to Automation Systems Specification","Description","Unit","Qty","Rate","Amount"]
[]
["E",null,"Automation Equipment"]
["E1",null,"Bill No.1"]
["E1.1",null,"Detail Design"]
["E1.1.1","3.1.1","Conformance to general specification requirements","Sum","Lot"]
["E1.1.2","3.2.1.1","Put into operation two (2) latest generation PLCs complete with all modules including Profibus module and ancillary items.","Sum","Lot"]
["E1.1.3","3.2.2.1","Put into operation one (1) PRM.","Sum","Lot"]
["E1.1.4","3.2.2.2","Put into operation two (2) OLMs (Profibus Optic Link Module) including connectors.","Sum","Lot"]
[null,"3.2.2.3",null,"Sum","Lot"]
[null,"3.2.3.1",null,"Sum","Lot"]
[null,"3.2.4.1",null,"Sum","Lot"]
[null,"3.2.5.1",null,"Sum","Lot"]
[null,"3.2.5.2",null,"Sum","Lot"]
[null,"3.2.6.1",null,"Sum","Lot"]
[null,"3.2.6.2",null,"Sum","Lot"]
[null,"3.2.6.3",null,"Sum","Lot"]
["E1.1.5","3.2.7.1","Deliver, off load, install, test, and commission two (2) galvanized kiosks from Central Depot stores to Vereeniging Pumping Station.","Sum","Lot"]
["E1.1.6","3.2.8.1",null,"Sum","Lot"]
["E1.1.7","3.2.9.1","Allow for complete length of 150mm heavy duty mesh cable trays, complete pieces of 150mm heavy duty mesh T pieces, complete pieces of 150mm heavy duty mesh 90 degree bends, complete length of 150mm heavy duty mesh droppers, complete length of 150mm heavy duty mesh risers and complete pieces of 150mm heavy duty mesh 4 way cross overs.","Sum","Lot"]
["E1.1.8","3.2.10.1","Supply all commissioning spares necessary to test and commission the installation","Sum","Lot"]
["E1.1.9","3.2.11.1","Supply all the maintenance spares necessary to maintain the installation done.","Sum","Lot"]
["E1.1.10","3.2.12.1","Develop the new PLC software.","Sum","Lot"]
["E1.1.11","3.2.13.1","Modify, test and commission the existing Engine room 4 Archestra based SCADA program","Sum","Lot"]
["E1.1.12","3.2.14.1","Log all selected tags as may be directed by the Engineer into an Historian server.","Sum","Lot"]
{"$rows_empty":7}
["E1.1.13",null,"All other  Equipment and actions not stated above which may be required to complete and commission the Installation (including risk mitigation and safety)"]
[null,null,"List below:"]
["E1.1.13.1",null,"1)"]
["E1.1.13.2",null,"2)"]
["E1.1.13.3",null,"3)"]
["E1.1.13.4",null,"4)"]
[]
[]
[]
[]
[null,null,"Schedule E1 Carried Forward",{"$nulls":3},0]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No","Refers"]
[]
["E2",null,"Bill No.2"]
["E2.1",null,"Manufacture Supply and Deliver"]
["E2.2",null,"Supply and Deliver two (2) PLC'S"]
["E2.3",null,"Supply and deliver one (1) PRM"]
["E2.4",null,"Supply and Deliver two (2)  OLMs (Profibus Optic Link Module) including connectors."]
["E2.5",null,"Supply and deliver one hundred (100)) meters of Profibus cable including connectors and accessories."]
["E2.6",null,"Supply and deliver complete length of seven way configured fibre tubes."]
["E2.7",null,"Supply and deliver complete length of category 6 STP cable."]
["E2.8",null,"Supply and deliver complete length of control and instrumentation wiring for sump pump signals."]
["E2.9",null,"Supply and deliver surge protection system on instrumentation cables."]
["E2.10",null,"Supply and deliver two (2) din rail UPS."]
["E2.11",null,"Supply and deliver four (4) 10A, 24VDC power supplies."]
["E2.12",null,"Supply and deliver two (2) diode bridge rated at 10A."]
["E2.13",null,"Deliver, off load, install, test, and commission two (2) galvanized kiosks from Central Depot stores to Vereeniging Pumping Station."]
["E2.14",null,"Manufacture supply and deliver three (3) fibre optic splice boxes."]
["E2.15",null,"Manufacture supply and deliver Allow for complete length of 150mm heavy duty mesh cable trays"]
{"$rows_empty":27}
[null,null,"Schedule E2 Carried Forward",{"$nulls":3},0]
[]
["Section E Carried Forward to Summary",{"$nulls":5},0]

{"sheet":"SCHEDULE F - CIVIL","index":7,"n_rows":362,"n_cols":7,"rows_kept":362,"merged":[[0,2,0,5],[1,2,1,4],[1,7,2,7],[6,1,7,1],[37,1,38,1],[127,0,127,2],[131,0,131,2],[174,0,174,2],[178,0,178,2],[276,0,276,2],[280,0,280,2]],"flags":["formulas_cached_only"]}
[null,null,"CONSTRUCTION OF THE CATHEDRAL HEADER CHAMBER AT"]
[null,null,"VEREENIGING PUMPING STATION",{"$nulls":3},"SCHEDULE G: CIVIL"]
[]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No","Refers"]
[]
["F1","SANS 1200 C","SECTION F1:  SITE CLEARANCE"]
[]
[]
[null,8.2,"SCHEDULED ITEMS"]
[]
["F1.1","8.2.1","Clear and grub","ha","0.1"]
[]
["F1.2","8.2.4","Reclear surfaces (only on instructions from the engineer)","ha","0.1"]
[]
["F1.3","8.2.9","Transport materials and debris to approved site (within a 20-30km radius) and dump ","m3.km",{"v":1000,"d":"1,000"}]
[]
["F1.4","8.2.8","Demolish and remove structures/buildings and dismantle steelwork, etc"]
[]
[null,null,"Demolition, dismantling and removal works to be phased-in line with an approved programme or shut down procedures. "]
[]
["F1.4.1",null,"i) Dismantle existing shed on Cathedral roof, and store for later re-instatement (as per RW Drawing R028765/001) (sum to include all required temporary works) ","Sum",{"v":1,"d":"1.0"}]
[]
["F1.4.2",null,"ii) Remove existing removable concrete covers over valves on Cathedral header roof, and store for later re-instatement (as per RW Drawing R028765/001) (sum to include all required temporary works)","Sum",{"v":1,"d":"1.0"}]
[]
["F1.4.3",null,"iii) Demolish existing roof slab and beam system as per the RW drawing R028765/001 and 002 (sum to include all required temporary works) (approximately 40m3 of at least 35 Mpa reinforced concrete)","Sum",{"v":1,"d":"1.0"}]
[]
["F1.5","8.2.9","Transport materials and debris to unspecified sites and dump (Provisional) (only debris identified as requiring disposal, as instructed by the Engineer)","t.km",{"v":4000,"d":"4,000"}]
[]
["F1.6","8.2.10","Remove topsoil to nominal depth of 150mm and stockpile (up a depth of 300mm)","m3",36]
[]
[]
[]
[null,null,"Sub-section F1 Total",{"$nulls":3},0]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No","Refers"]
[null,null,"SANS 1200DA: Earthworks (Small Works)"]
["F2","SANS 1200 DA","SECTION F2:  EARTHWORKS"]
[]
[]
[null,8.3,"SCHEDULED ITEMS"]
[]
["F2.1","8.3.1","Excavation"]
[]
["F2.1.1",null,"b) Excavate in all materials and use for backfill (In-situ backfill of selected suitable material from excavations, compacted in layers not exceeding 150mm to 93% MOD AASHTO density at -1% to +2% OMC) or dispose, as ordered (excluding shoring)","m3",890]
[]
[null,null,"c) Extra-over for:"]
[]
["F2.1.2",null,"1) Hard excavation (where required)","m3",267]
[]
["F2.2","8.3.4","Importing of  material from a commercial source"]
[]
["F2.2.1",null,"i) Importing of backfill G7 Material compacted in layers not exceeding 150mm in thickness compacted to 93% MOD AASHTO density AT -1% to +2% OMC","m3",150]
[]
["F2.2.2",null,"ii) Importing of G3 backfill material (as per DRG R028765/100)","m3",350]
[]
["F2.2.3",null,"iii) G5 Material compacted in layers not exceeding 100 mm in thickness compacted to 95% MOD AASHTO density AT -1% to +2% OMC","m3",30]
[]
["F2.2.4",null,"iv) C3 Material compacted to 96% MOD AASHTO at OMC (5% cement of total fill volume)","m3",14]
[]
["F2.2.5",null,"v) 20mm layer of sand underneath the paving blocks","m2",61]
[]
["F2.3","8.3.5","Existing services (exposure, protection and alteration)","m2",200]
[]
["F2.4","8.3.6","Topsoiling","m2",65]
[]
["F2.5","8.3.8","Traffic signs","Sum",1]
[]
["F2.6","8.3.9","Shoring of excavations (the proposed works are to be carried out in a confined environment with numerous services obstructing the construction works, therefore the Contractor is expected to price for Vertical excavations and appropriate shoring for the chamber illustrated on RW Drawing R028765/100 - reference should be made to the technical specifications)","Sum",1]
[]
["F2.7","8.3.10","Soil Testing"]
[]
["F2.7.1",null,"i) Foundation Indicator / Soil Classification","Sum",1]
[]
["F2.7.2",null,"ii) Field Dry Density","Sum",1]
[]
["F2.7.3",null,"iii) Modified AASHTO Maximum Dry Density","Sum",1]
[]
["F2.7.4",null,"iv) Additional testing as may be required by the Engineer","Prov. Sum",1]
[]
[]
[null,null,"Sub-section F2 Total",{"$nulls":3},0]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No","Refers"]
[]
["F3","SANS 1200 GA","SECTION F3: CONCRETE WORKS (STRUCTURAL) "]
[]
["F3.1","8.2","SCHEDULED FORMWORK ITEMS"]
[null,null,"Supply all materials, install and remove formwork (rate to include for forming of 20 x 20 chamfers to all exposed edges for:)"]
[]
["F3.1.2","8.2.2","Smooth"]
[]
[null,null,"i) Isolation Valve Chamber "]
[]
["F3.1.2.1",null,"1) Walls","m²",476]
[]
["F3.1.2.2",null,"2) Underside of Roof Slab ","m²",35]
[]
["F3.1.3","8.2.3","Narrow Widths"]
[]
[null,null,"i) Isolation Valve Chamber "]
[]
["F3.1.3.1",null,"1) Sides of roof slab (300mm high)","m",30]
[]
["F3.1.3.2",null,"2) Sides of base slab (600mm high)","m",35]
[]
["F3.1.3.3",null,"3) Sides of downstand portion of the beam (150mm high)","m",51]
[]
["F3.1.4","8.2.4","Box out Holes / Form Voids"]
[]
["F3.1.4.1",null,"i) Chamber - box out hole for 2500mm x 2500mm x 500mm thick","No.",4]
[]
["F3.1.4.2",null,"ii) Box out hole for 500mm x 500mm x 300mm (to sump)","No.",1]
[]
["F3.2","8.3","SCHEDULED REINFORCEMENT ITEMS"]
[]
["F3.2.1","8.3.1","Steel bars"]
[]
[null,null,"i) Mild steel reinforcement"]
[]
["F3.2.1.1",null,"1) Isolation Valve Chamber ","kg",2839]
[]
[null,null,"ii) High tensile steel reinforcement"]
[]
["F3.2.1.2",null,"1) Isolation Valve Chamber ","kg",28390]
[]
[]
["Total Carried Forward ",{"$nulls":5},0]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No","Refers"]
[]
["Total brought forward ",{"$nulls":5},0]
[]
["F3.3","8.4","SCHEDULED CONCRETE ITEMS"]
[]
["F3.3.1","8.4.2","Blinding Layer in … Concrete …"]
[]
[null,null,"i) 50mm Class 15/19 MPa Blinding Layer:"]
[]
["F3.3.1.1",null,"1) Isolation Valve Chamber ","m2",65]
[]
["F3.3.2","8.4.3","Strength Concrete, Grade ..."]
[]
[null,null,"i) Grade 35MPa/19mm:"]
[]
["F3.3.2.1",null,"1) Isolation Valve Chamber","m3",167]
[]
["F3.3.3","8.4.4","Unformed Surface Finishes"]
[]
["F3.3.3.1",null,"a) Wood-floated finish to floor and roof slabs","m2",110]
[]
["F3.4",8.5,"JOINTS"]
[]
["F3.4.1",null,"i) Expansion joints between Isolation valve chamber precast roof panels as per drawing Rand Water drawing RO28765/001) (Joint to be SIKAFLEX CONSTRUCTION + or similar approved)","m",50]
[]
["F3.4.2",null,"ii) Isolation joints between Isolation Valve chamber cast in-situ roof slab and removable roof panels as per drawing Rand Water drawing RO28765/100-101)  (Joint to be SIKAFLEX CONSTRUCTION + or similar approved)","m",25]
[]
["F3.5",8.6,"MANUFACTURE (OR SUPPLY) AND ERECT PRECAST ELEMENTS"]
[]
[null,null,"i) Manufacture, deliver and erect precast concrete elements as per drawings R028765/001-004 and R028765/100-101 and the technical specifications"]
[]
["F3.5.1",null,"1) Header Precast Concrete Roof Elements (approximately 142 square meters of 255mm 40MPa hollow core slab for all 9 items)","m3",30]
[]
["F3.5.2",null,"2) 2000mm Long x 610mm width x 1220mm High precast Alfabloc barrier wall (See DRG No. R028765/100-101)","No.",7]
[]
["F3.5.3",null,"3) Concrete kerbing (Figure 8 (a))","m",45]
[]
["F3.5.4",null,"4) Concrete paving blocks complete (60 S-C) (Laid in Herringbone pattern)","m2",61]
[]
["F3.6",8.7,"Grouting"]
[]
["F3.6.1",null,"i) Under bases (under structural steel walkways to be reinstated at the cathedral header) - 60 MPa self leveling grout","m3",{"v":0.5,"d":"1"}]
[]
[]
["Total Carried Forward ",{"$nulls":5},0]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No","Refers"]
[]
["Total brought forward ",{"$nulls":5},0]
[]
["F3.7","8.8","MISCELLANEOUS "]
[]
["F3.7.1",null,"i) Cast in PVC sleeves:"]
[]
["F3.7.1.1",null,"1) 50mm diameter x 380mm long","No.",8]
[]
["F3.7.1.2",null,"2) 240mm diameter x 300mm long for T-piece air ventilation pipes with embeded flange (see DRG No. B4141)","No.",5]
[]
["F3.7.1.3",null,"ii) Supply and cast in standard Rand Water frame and sump cover","No.",1]
[]
["F3.7.1.4",null,"iii) Cast in standard Rand Water manhole frame and cover (supplied by Rand Water)","No.",1]
[]
["F3.7.1.5",null,"iv) Supply and install standard Rand Water grab rail","No.",1]
[]
["F3.7.1.6",null,"v) Making good of all damaged components of the IBR roof hut entrance structure for reuse and paint to match existing"," Prov. Sum",1,30000,30000]
[]
["F3.7.1.8",null,"Contractors mark-up on item F3.7.1.6 above","%",30000]
[]
["F3.7.1.9",null,"vi) Water proofing compound - \"Sika Cemflex\" 1m wide rolls fabric: 20m*150mm OR similar Approved (All around) applied in strict accordance with manufacture's specifications","Sum",1]
[]
["F3.7.1.10",null,"vii) Supply and install Fibre Reinforced Plastic grating (see details on Drg. No. RO28765/100-101)","m2",14]
[]
["F3.7.1.11",null,"viiI) Supply and install 16mm diameter holding down bolts for the Actuators (see details on Drg. No. R028765/100-101)","No.",8]
[]
["F3.7.1.12",null,"ix) Supply and install 229mm ID T-piece air ventilation pipe fitted with a 10mm thick paddle flange (see details on Drg. No. RO28765/100-101 and B4141)","No.",5]
[]
["F3.8","-","Supply and install standard Rand Water internal catladder consisting of Fibre Reinforced Plastic material (refer to drawings No. A. 7406 and R028765/100-101 for catladder lengths)\n"]
[]
["F3.8.1",null,"  i) 8.1m high (fitted with safety cage)","No.",1]
[]
["F3.8.2",null,"  ii) 4.7m high ","No.",1]
[]
["F3.9","-","Flo-drain system"]
[null,null,"(Refer to specification)"]
[]
["F3.9.1",null,"i) Supply and installation of the flo-drain system with geopipe (refer to DRG No. RO28765/100-101)","Sum",1]
[]
["F3.9.2",null,"ii) Supply and placing of Bidim cloth around the drainable material (refer to DRG No. RO28765/100-101)","m2",290]
[]
["F3.10",8.9,"Concrete Cube Testing"]
[]
["F3.10.1",null,"i) Testing of concrete","No.",270]
[]
["F3.10.2",null,"ii) Supply cube testing machine on site with recent calibration certified and water trough","Sum",1]
[]
["F3.11","8.10","Curing"]
[]
["F3.11.1",null,"i) Curing of concrete","Sum",1]
[]
["F3.12","8.11","Water Tightness Testing"]
[]
["F3.12.1",null,"i) Isolation Valve Chamber and Chamber Roof","Sum",1]
[]
["F3.12.2",null,"ii) Header Roof","Sum",1]
[]
[]
[]
[null,null,"Sub-section F3 Total",{"$nulls":3},{"v":30000,"d":"R 30,000.00"}]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No","Refers"]
[]
["F4","SANS 1200H","SECTION F4: STRUCTURAL STEELWORK "]
[]
["F4.1","8.3","SCHEDULED ITEMS"]
[]
["F4.1.1","8.3.1","Supply and Fabrication"]
[]
[null,"8.3.1.1","Preparation of shop detail drawings"]
[]
["F4.1.1.1",null,"i) Structural Steelworks as per drawing R028765/001 and 002","Sum",1]
[]
["F4.1.1.2",null,"ii) Frames for walkway (as per drawing RO28765/100-101) - excluding grating","Sum",1]
[]
[null,"8.3.1.2","Supply and fabrication of steelwork"]
[]
["F4.1.1.3",null,"i) Structural Steelworks as per drawing R028765/001 and 002 (305x305x118 and 305x305x158 beams)","t",7]
[]
["F4.1.1.4",null,"ii) Frames for walkway (as per drawing RO28765/100-101) - excluding grating","t",1]
[]
["F4.1.2","8.3.2","Delivery to Site"]
[]
[null,"8.3.2.1.","Normal Delivery"]
[]
["F4.1.2.1",null,"i) Structural Steelworks as per drawing R028765/001 and 002","t",7]
[]
["F4.1.2.2",null,"ii) Flooring Complete and Installed with Frames (as per drawing RO28765/100-101) - excluding grating","t",1]
[]
["F4.1.3","8.3.3","Erection on Site"]
[]
["F4.1.3.1",null,"i) Re-instatement of Cathedral Header roof Hut dismantled during construction (as per drawing R028765/001)","Sum",1]
["F4.1.3.2"]
[null,null,"ii) Structural Steelworks as per drawing R028765/001 and 002","Sum",1]
[]
["F4.1.3.3",null,"iii) Frames for walkway (as per drawing RO28765/100-101) - excluding grating","Sum",1]
[]
[]
["Total Carried Forward ",{"$nulls":5},0]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No","Refers"]
[]
["Total brought forward ",{"$nulls":5},0]
[]
[]
["F4.1.4","8.3.6","Holding Down Bolts"]
[]
["F4.1.4.1",null,"i) Structural Steelworks as per drawing R028765/001 and 002","t",0.2]
[]
["F4.1.4.2",null,"ii) Frames for walkway (as per drawing RO28765/100-101) - excluding grating","t",0.1]
[]
["F4.1.5","8.3.7","Handrails"]
[]
["F4.1.5.1",null,"Handrail assembly complete (see DRG No, R028765/100-101)","Sum",1]
[]
["F4.1.6","8.3.10","Non-destructive Testing"]
[]
["F4.1.6.1",null,"i) Structural Steelworks as per drawing R028765/001 and 002","Sum",1]
[]
["F4.1.6.2",null,"ii) Frames for walkway (as per drawing RO28765/100-101) - excluding grating","Sum",1]
[]
["F4.1.7","8.3.12","Additional Items"]
[]
["F4.1.7.1",null,"i) Additional steel bolts, gusset plates and members required for the construction and erection of steel and FRP elements - the rate should include the manufacture, corrosion protection (by galvanizations as per the project specification), delivery, and installation of all steel elements","t",{"v":0.30000000000000004,"d":"0.3"}]
{"$rows_empty":15}
[null,null,"Sub-section F4 Total",{"$nulls":3},0]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No","Refers"]
[]
["F5","SANS 1200HC","SECTION F5: Corrosion Protection of Structural Steelwork"]
[]
[null,null,"All structural steel to be Hot Dipped Galvanized to the requirements of SANS 763"]
[]
["F5.1",8.2,"SCHEDULED ITEMS"]
[]
["F5.1.1","8.2.1","Surface Dressing and Repairs at Place of Fabrication"]
[]
["F5.1.1.1",null,"i) Structural Steelworks as per drawing R028765/001 and 002","t",7]
[]
["F5.1.1.2",null,"ii) Frames for walkway (as per drawing RO28765/100-101) - excluding grating","t",1]
[]
["F5.1.2","8.2.2","Transport"]
[]
["F5.1.2.1",null,"i) Structural Steelworks as per drawing R028765/001 and 002","t",7]
[]
["F5.1.2.2",null,"ii) Frames for walkway (as per drawing RO28765/100-101) - excluding grating","t",1]
[]
["F5.1.3","8.2.3","Surface Preparation and Coating Application"]
[]
["F5.1.3.1",null,"a) in the shop"]
[]
["F5.1.3.1.1",null,"i) Structural Steelworks as per drawing R028765/001 and 002","t",7]
[]
["F5.1.3.1.2",null,"ii) Frames for walkway (as per drawing RO28765/100-101) - excluding grating","t",1]
{"$rows_empty":13}
[null,null,"Sub-section F5 Total",{"$nulls":3},0]
[]
[null,null,"Section F Carried Forward to Summary",{"$nulls":3},{"v":30000,"d":"R 30,000.00"}]

{"sheet":"SCHEDULE G - ELECTRICAL","index":8,"n_rows":416,"n_cols":7,"rows_kept":416,"merged":[[0,4,0,6],[1,1,1,6],[2,9,2,11],[3,4,3,6],[3,9,3,11],[5,0,6,0],[5,1,6,1],[5,2,6,2],[5,3,6,3],[5,4,6,4],[5,5,6,5],[5,6,6,6],[7,0,8,0],[7,1,8,1],[7,2,8,2],[7,3,10,6],[21,0,27,0],[21,1,27,1],[21,3,27,3],[21,4,27,4],[21,5,27,5],[21,6,27,6],[28,2,28,5],[29,0,29,4],[30,3,31,6],[47,0,47,2],[48,0,48,4],[67,0,67,2],[68,0,68,4],[91,0,91,2],[92,0,92,4],[122,0,122,2],[123,0,123,4],[152,0,152,2],[153,0,153,4],[166,0,172,0],[166,1,172,1],[166,3,172,3],[166,4,172,4],[166,5,172,5],[166,6,172,6],[173,2,173,5],[181,0,181,2],[182,0,182,4],[205,0,205,2],[206,0,206,4],[220,0,226,0],[220,1,226,1],[220,3,226,3],[220,4,226,4],[220,5,226,5],[220,6,226,6],[227,2,227,5],[237,0,237,2],[238,0,238,4],[257,0,257,2],[258,0,258,4],[289,0,289,2],[290,0,290,4],[319,0,319,2],[320,0,320,4],[352,0,352,2],[353,0,353,4],[360,0,365,0],[360,1,365,1],[360,3,365,3],[360,4,365,4],[360,5,365,5],[360,6,365,6],[366,2,366,5],[382,0,382,2],[383,0,383,4],[398,0,404,0],[398,1,404,1],[398,3,404,3],[398,4,404,4],[398,5,404,5],[398,6,404,6],[405,2,405,5],[406,2,407,6],[414,2,414,6],[415,2,415,5]],"flags":["formulas_cached_only"]}
[{"$nulls":4},"TENDER NO. xxxxxxxxxx / xx"]
[null,"       TENDER FOR THE DESIGN, MANUFACTURE, SUPPLY, DELIVERY, INSTALLATION, CONSTRUCTION, CONFIGURATION, TESTING AND COMMISSSIONING OF AN ELECTRICAL & SMALL POWER AND LIGHTING INSTALLATION AND ASSOCIATED \nWORKS AT THE VEREENIGING CATHEDRAL HEADER AND ENGINE ROOM 4 VALVE ISOLATION \nCHAMBERS\n"]
[]
[{"$nulls":4},"Schedule G: Electrical"]
[]
["Item   No.","Payment Refers","Description","Unit","Qty","Rate","Amount"]
[]
[null,null,"Electrical Equipment and Works As Per System Specifications, Drawing & Legends"]
[]
[null,null,"BILL No.1"]
["G1","1 & 2","DETAILED DESIGN"]
[null,null,"Design all items forming part of the electrical and  small power and lighting installation including, the incoming power supplies, cable installation, calculations, drawings and documents, as-built (record) drawings, close-out reports and manuals"]
[null,"1,2,4,5,6,7 & 8"," Power Supply and Distribution Design"]
["G1.1",null,"Provision for the designs of two power distribution kiosks, two small power and lighting distribution boards, three sump pump control panels, one extraction fan control panel and nine valve isolation panels complete with hot dipped galvanized stands and GA’s to be approved prior to manufacturing","Sum",1]
[null,"1,2 & 9","Small Power and Lighting Design"]
["G1.2",null,"Provision for the designs of a small power and lighting system in order to comply with National standards and legislation complete with pre installation lux level design and post lux level report on completion of installation. Minimum of 320 Lux to be achieved in both chambers on the walkways. Also make provision for emergency backed-up light fittings as dictated by legislation.","Sum",1]
[null,"1,2,10,11,12 & 13","Power and Control Cabling"]
["G1.3",null,"Provision for the designs of all cable and cable support systems complete with calculations and layout drawings to be approved by Rand Water. ","Sum",1]
[null,"1 & 2","Interface to Architectural, Civil/Structural, Automation, IT and Mechanical Requirements"]
["G1.4",null,"Provision for all interface requirements between various disciplines as part of the design stage ","Sum",1]
[null,"All clauses","Additional Works Not Specifically Listed"]
["G1.5",null,"Provide the details of any additional design items not specifically mentioned for these entrances, that might be required for a complete and working installation. If no details are provided below, any additional items required to complete the works shall be supplied, installed and commissioned at the contractors' cost. No further claims shall  be allowed on this item.","Sum",1]
[null,null,1]
[null,null,2]
[null,null,3]
[null,null,4]
[null,null,5]
[null,null,6]
[null,null,"Schedule G1 Carried Forward",{"$nulls":3},"R"]
["SCHEDULE G1 BROUGHT FORWARD ",{"$nulls":5},"R"]
[null,null,"BILL No.2"]
["G2",null,"MANUFACTURE, SUPPLY AND TEST"]
[null,null,"Electrical installation and items forming part of the electrical and small power and lighting installation (and all building components) in accordance with the functional requirements, approved designs, drawings and schematics. "]
[null,"1 & 3","Modifications and Additions at Wash Water Power Supply Source"]
["G2.1",null,"Provision for the supply of an 125 amp 400 volt 36 kA circuit breaker with adjustable IDMT unit up to 1000 mA, in the emergency section of the 400 Volt MCC to supply new Kiosk no.1 complete with all cabling  and accessories for a complete installation.","Sum",1]
["G2.2",null,"Provision for the supply of a 63 amp 400 volt 36 kA breaker  with adjustable IDMT unit up to 1000 mA, in the emergency section of the 400 Volt MCC to supply new Kiosk no.2 complete with all accessories for a complete installation.","Sum",1]
[null,"1,4,5,6,7 & 8","Power Supply and Distribution"]
["G2.3",null,"Provision for a new 400 volt 3CR12 SS orange powder coated IP65 rated outdoor kiosk no.1 complete with all circuit breakers, equipment, engraved labels and galvanized steel pedestal frame.","Sum",1]
["G2.4",null,"Provision for the factory acceptance testing of Kiosk no.1","Sum",1]
["G2.5",null,"Provision for a new 400 volt 3CR12 SS orange powder coated IP65 rated outdoor kiosk no.2 complete with all circuit breakers, equipment, engraved labels and galvanized steel pedestal frame. ","Sum",1]
["G2.6",null,"Provision for the factory acceptance testing of Kiosk no.2","Sum",1]
["G2.7",null,"Provision for a new 400 volt 3CR12 SS orange powder coated IP65 rated outdoor small power and distribution board at the Cathedral Header Chamber complete with all circuit breakers, equipment, engraved labels and galvanized steel pedestal frame.","Sum",1]
["G2.8",null,"Provision for the factory acceptance testing of the SP&L distribution board at the Cathedral header chamber.","Sum",1]
["G2.9",null,"Provision for a new 400 volt 3CR12 SS orange powder coated IP65 rated outdoor small power and distribution board at Engine Room no.4 valve isolation chamber complete with all circuit breakers, equipment, engraved labels and galvanized steel pedestal frame.","Sum",1]
["G2.10",null,"Provision for the factory acceptance testing of the SP&L distribution board for the Engine Room no. 4 chamber","Sum",1]
[]
[]
["Total Carried Forward ",{"$nulls":5},"R"]
["Total brought forward",{"$nulls":5},"R"]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No","Refers"]
[]
["G2.11",null,"Provision for two new 400 volt 3CR12 SS orange powder coated IP65 rated outdoor Sump pump control panels at the Cathedral Header Chamber complete with all circuit breakers, equipment, engraved labels and galvanized steel pedestal frame .(float switches covered elsewhere)","Sum",1]
["G2.12",null,"Provision for the factory acceptance testing of the sump pump control panels at the Cathedral Header","Sum",1]
["G2.13",null,"Provision for a new 400 volt 3CR12 SS orange powder coated IP65 rated outdoor Sump pump control panel at Engine Room no.4 valve isolation chamber complete with all circuit breakers, equipment, engraved labels and galvanized steel pedestal frame.(float switches covered elsewhere","Sum",1]
["G2.14",null,"Provision for the factory acceptance testing of the sump pump control panels at the Engine Room no. 4 chamber","Sum",1]
["G2.15",null,"Provision for a new 400 volt 3CR12 SS orange powder coated IP65 rated outdoor Extraction fan control panel at the Cathedral Header Chamber complete with all circuit breakers, equipment, engraved labels and galvanized steel pedestal frame.","Sum",1]
["G2.16",null,"Provision for the factory acceptance testing of the extraction Fan control panel at the Cathedral Header","Sum",1]
["G2.17",null,"Provision for seven  new 400 volt 3CR12 SS orange powder coated IP65 rated outdoor valve isolation  panels close to each of the actuators at the Cathedral Header Chamber complete with all circuit breakers, equipment, engraved labels and galvanized steel pedestal frames.","Sum",1]
["G2.18",null,"Provision for the factory acceptance testing of the isolation valve control panels at the Cathedral Header","Sum",1]
["G2.19",null,"Provision for two  new 400 volt 3CR12 SS orange powder coated IP65 rated valve isolation  panels close to each actuator at the Engine Room no.4 valve isolation chamber complete with all circuit breakers, equipment, engraved labels and galvanized steel pedestal frame.","Sum",1]
["G2.20",null,"Provision for the factory acceptance testing of the isolation valve control panels at the Engine Room no. 4 chamber","Sum",1]
[null,"1,10,11, 12 & 13","Power and Control Cabling"]
["G2.21",null,"50mm² x 4 core Cu PVC SWAPVCPVC  power supply cable between 400 Volt MCC emergency section and Kiosk no.1 situated at the Cathedral Header Chamber ","m",150]
["G2.22",null,"25mm² x 4 core Cu PVC SWAPVCPVC  power supply cable between 400 Volt MCC emergency section and Kiosk no.2 situated at the Engine Room Valve Isolation Chamber","m",150]
[]
[]
["Total Carried Forward ",{"$nulls":5},"R"]
["Total brought forward",{"$nulls":5},"R"]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No","Refers"]
[]
["G2.23",null,"16mm² x 4 core Cu PVC SWAPVCPVC cable between kiosk no.1 and the SP&L distribution board at Cathedral Header Chamber","m",5]
["G2.24",null,"4mm² x 3 core Cu PVC SWAPVCPVC cable between the SP&L distribution board  and the first socket outlet at Cathedral Header Chamber","m",10]
["G2.25",null,"2.5mm² x 3 core Cu PVC SWAPVCPVC cable between the SP&L distribution board  and the first light switch at Cathedral Header Chamber","m",15]
["G2.26",null,"10mm² x 4 core Cu PVC SWAPVCPVC cable between kiosk no.1 and the two Sump pump control panels at Cathedral Header Chamber","m",50]
["G2.27",null,"4mm² x 4 core Cu PVC SWAPVCPVC cable between the two Sump pump control panels and each sump pump at Cathedral Header Chamber.","m",40]
["G2.28",null,"1.5mm² x 7 core Cu PVC SWAPVCPVC cable between the two Sump pump control panels and each sump pump level switches termination boxes at Cathedral Header Chamber.","m",40]
["G2.29",null,"4mm² x 4 core Cu PVC SWAPVCPVC cable between kiosk no.1 and the Extraction Fan control panel at Cathedral Header Chamber.","m",40]
["G2.30",null,"4mm² x 4 core Cu PVC SWAPVCPVC cable between the Extraction Fan control panel and the Extraction Fan at Cathedral Header Chamber.","m",5]
["G2.31",null,"10mm² x 4 core Cu PVC SWAPVCPVC cable between kiosk no.1 and each one of the seven Valve Isolation panels at the Cathedral Header actuators.","m",170]
["G2.32",null,"6mm² x 4 core Cu PVC SWAPVCPVC cable between each of the seven actuator valve isolation panels and each actuator at the Cathedral Header.","m",30]
["G2.33",null,"16mm² x 4 core Cu PVC SWAPVCPVC cable between kiosk no.2 and the SP&L distribution board at Engine Room 4 Isolation Chamber","m",5]
["G2.34",null,"2.5mm² x 3 core Cu PVC SWAPVCPVC cable between the SP&L distribution board  and the first light switch at Engine Room 4 Isolation Chamber ","m",15]
["G2.35",null,"10mm² x 4 core Cu PVC SWAPVCPVC cable between kiosk no.2 and the Sump pump control panel at Engine Room 4 Isolation Chamber","m",15]
["G2.36",null,"4mm² x 4 core Cu PVC SWAPVCPVC cable between the Sump pump control panel and the sump pump at Engine Room 4 Isolation Chamber.","m",40]
["G2.37",null,"1.5mm² x 7 core Cu PVC SWAPVCPVC cable between the Sump pump control panel and the sump pump level switches termination boxes at Engine Room 4 Isolation Chamber.","m",40]
["G2.38",null,"10mm² x 4 core Cu PVC SWAPVCPVC cable between kiosk no.2 and each one of the two Valve Isolation panels at the Engine Room 4 Isolation Chamber actuators.","m",50]
["G2.39",null,"6mm² x 4 core Cu PVC SWAPVCPVC cable between each of the two valve isolation panels and each actuator at the Engine Room 4 Isolation Chamber.","m",6]
[]
[]
["Total Carried Forward ",{"$nulls":5},"R"]
["Total brought forward",{"$nulls":5},"R"]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No","Refers"]
[]
[null,"1,10,11, 12 & 13","Cable Terminations"]
[null,null,"Includes SANS approved metal type glands, PVC shrouds, lugs and any other material required for a complete installation"]
["G2.40",null,"50mm² x 4 core Cu PVC SWAPVCPVC cable","No",2]
["G2.41",null,"25mm² x 4 core Cu PVC SWAPVCPVC cable","No",2]
["G2.42",null,"16mm² x 4 core Cu PVC SWAPVCPVC cable","No",4]
["G2.43",null,"10mm² x 4 core Cu PVC SWAPVCPVC cable","No",22]
["G2.44",null,"6mm² x 4 core Cu PVC SWAPVCPVC cable","No",18]
["G2.45",null,"4mm² x 3 core Cu PVC SWAPVCPVC cable","No",2]
["G2.46",null,"2.5mm² x 3 core Cu PVC SWAPVCPVC cable","No",4]
["G2.47",null,"1.5mm² x 7 core Cu PVC SWAPVCPVC cable","No",4]
[null,"1,10,11, 12,13 & 14","Earth Conductors "]
["G2.48",null,"25mm² Cu equivalent  Anti-theft type copper coated metal clad steel earth conductor for kiosk no.1","m",150]
["G2.49",null,"16mm² Cu equivalent  Anti-theft type copper coated metal clad steel earth conductor for kiosk no.2","m",150]
["G2.50",null,"6mm² black insulated copper earth conductor to run with power supply cabling for all other control panels and distribution boards","m",450]
["G2.51",null,"Earth conductors for all bonding and earthing requirements ","Sum",1]
[null,"1,10,11, 12,13 & 14","Terminations for Earth Conductors complete with SABS approved lugs and shrouds."]
["G2.52",null,"25mm² Cu equivalent  Anti-theft type copper coated metal clad steel earth conductor for kiosk no.1 ","No",2]
["G2.53",null,"16mm² Cu equivalent  Anti-theft type copper coated metal clad steel earth conductor for kiosk no.2 ","No",2]
["G2.54",null,"6mm² black insulated copper earth conductor for all other control panels and distribution boards ","No",32]
["G2.55",null,"Terminations for all Earth conductors for all bonding and earthing requirements ","Sum",1]
[null,"1,10,11, 12,13 & 14","Site Works for Cable Installation"]
["G2.56",null,"Provide for water, UV and corrosion resistant modular type cable sealing system at all cable entries into concrete chambers complete with core drilling where required(no resin or foam type allowed)","Sum",1]
["G2.57",null,"Sifted soil to be utilized for PVC sleeve bedding inside cable trench excavation (100mm below cable and 150mm above cable)","Sum",1]
["G2.58",null,"SABS approved Danger tape 200mm above cable on entire length of excavation","Sum",1]
[]
[]
["Total Carried Forward ",{"$nulls":5},"R"]
["Total brought forward",{"$nulls":5},"R"]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No","Refers"]
[]
["G2.59",null,"Cable route markers shall consist of concrete blocks with a concrete strength of at least 25 MPa, in the shape of truncated pyramid, approximately 300 mm high, 150 x 150 mm at the top and 250 x 250 mm at the bottom Aluminium plates shall be cast into the top of the blocks in such a manner that they cannot be pried loose. Power cable details and direction to be indicated on plate.","No",5]
["G2.60",null,"110mm PVC sleeves for underground use to house the electrical cabling","m",24]
["G2.61",null,"110mm PVC sleeve termination ends, joints, bends and end caps for electrical sleeves","Sum",1]
["G2.62",null,"SABS approved hot dipped galvanized cable rack/ ladders for a complete cable installation complete with cable rack/ ladder covers.","Sum",1]
["G2.63",null,"SABS approved hot dipped galvanized cable rack/ ladder pre-manufactured joints, bends and supports for a complete cable installation complete with cable rack/ ladder covers and fixings.","Sum",1]
[null,"1 & 9","Conduits and Power Systems"]
["G2.64",null,"25mm SABS approved surface mounted galvanized conduit for small power and lighting installations at the Cathedral Header Chamber.","Sum",1]
["G2.65",null,"25mm galvanized conduit loop in boxes, termination boxes, covers, couplings, bends, adaptors and supports for a complete installation at the Cathedral Header Chamber.","Sum",1]
["G2.66",null,"25mm SABS approved surface mounted galvanized conduit for small power and lighting installations at the Engine Room 4 Isolation Chamber.","Sum",1]
["G2.67",null,"25mm galvanized conduit loop in boxes, termination boxes, covers, couplings, bends, adaptors and supports for a complete installation at the Engine Room 4 Isolation Chamber.","Sum",1]
[null,"1 & 9","Socket Outlets, Switches and Isolators"]
["G2.68",null,"230 volt 16 amp IP65 rated surface mounted socket outlet ","No",6]
["G2.69",null,"230 volt IP65 rated surface mounted single lever light switch ","No",2]
["G2.70",null,"400 volt 3pole 60 amp IP65 rated surface mounted isolator at sump pump ","No",3]
["G2.71",null,"400 volt 3pole 60 amp IP65 rated surface mounted isolator at extraction fan","No",1]
["G2.72",null,"400 Volt 32 Amp IP65 rated welding socket outlet complete with male socket","No",2]
[null,"1 & 7","Sump Pump Level Float Switches"]
["G2.73",null,"24 Volt DC IP 65 adequately rated SABS approved  level control switches ","No",6]
[null,"1 & 9","General Purpose Insulated Conductors"]
["G2.74",null,"2.5mm² General Purpose insulated wire(phases + earth)","Sum",1]
["G2.75",null,"4mm² General Purpose insulated wire(phases + earth)","Sum",1]
[null,"1 & 9","Luminairs"]
["G2.76",null,"SABS approved 230 Volt IP 65 rated 75 watt wide beam LED type flood light complete with mounting bracket. (level of 320 Lux to be achieved). Complete with two spare fittings","Sum",1]
[]
[]
["Total Carried Forward ",{"$nulls":5},"R"]
["Total brought forward",{"$nulls":5},"R"]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No","Refers"]
[]
["G2.77",null,"SABS approved 230 Volt IP 65 rated 75 watt wide beam LED type emergency  flood light complete with batteries and mounting bracket. (level of 320 Lux to be achieved)Complete with two spare fittings","Sum",1]
["G2.78",null,"SABS approved 230 Volt IP 65 rated 46 watt 1200mm LED type vapour proof light fitting (level of 320 Lux to be achieved)Complete with two spare fittings","Sum",1]
["G2.79",null,"SABS approved 230 Volt IP 65 rated 46 watt 1200mm LED type emergency vapour proof light fitting complete with batteries (level of 320 Lux to be achieved)Complete with two spare fittings","Sum",1]
["G2.80",null,"SABS approved 230 Volt IP 65 rated 7 watt green EXIT LED type  light fitting complete with internal batteries, mounting brackets and relevant pictogram. Complete with two spare fittings ","Sum",1]
[null,1,"Miscellaneous Items"]
["G2.81",null,"Engraved labels for each isolator, socket outlet, light switch and distribution board ","Sum",1]
["G2.82",null,"Provide for all wire numbers and WKS cable labels.","Sum",1]
["G2.83",null,"Provide for Interface to Architectural, Mechanical, Automation and Civil/Structural requirements under this bill item","Sum",1]
["G2.84",null,"Provision for supervision  under this Bill item","Sum",1]
["G2.85",null,"Provide the details of any additional manufacture, supply and test items not specifically mentioned, that might be required for a complete and working installation. If no details are provided below, any additional items required to complete the works shall be supplied, installed and commissioned at the contractors' cost. No further claims shall  be allowed on this item.","Sum",1]
[null,null,1]
[null,null,2]
[null,null,3]
[null,null,4]
[null,null,5]
[null,null,6]
[null,null,"Schedule H2 Carried Forward",{"$nulls":3},"R"]
[null,null,"BILL No.3"]
["G3","1,3,4,5,6,7,,8,9,10,11,12,13,14 & 15","DELIVERY OF EQUIPMENT"]
["G3.1",null,"Deliver a 125 amp 400 volt 36 kA circuit breaker with adjustable IDMT unit up to 1000 mA, in the emergency section of the 400 Volt MCC to supply new Kiosk no.1 complete with all cabling  and accessories for a complete installation.","Sum",1]
["G3.2",null,"Deliver a 63 amp 400 volt 36 kA breaker  with adjustable IDMT unit up to 1000 mA, in the emergency section of the 400 Volt MCC to supply new Kiosk no.2 complete with all accessories for a complete installation.","Sum",1]
["G3.3",null,"Deliver new 400 volt 3CR12 SS orange powder coated IP65 rated outdoor kiosk no.1 & kiosk no.2 complete with all circuit breakers, equipment, engraved labels and galvanized steel pedestal frame.","Sum",1]
[]
[]
["Total Carried Forward ",{"$nulls":5},"R"]
["Total brought forward",{"$nulls":5},"R"]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No","Refers"]
[]
["G3.4",null,"Deliver new 400 volt 3CR12 SS orange powder coated IP65 rated outdoor small power and distribution board at the Cathedral Header Chamber  and Engine Room 4 Chamber complete with all circuit breakers, equipment, engraved labels and galvanized steel pedestal frame.","Sum",1]
["G3.5",null,"Deliver new 400 volt 3CR12 SS orange powder coated IP65 rated outdoor Sump pump control panels at the Cathedral Header Chamber and Engine Room no.4 Chamber complete with all circuit breakers, equipment, engraved labels and galvanized steel pedestal frame .(float switches covered elsewhere)","Sum",1]
["G3.6",null,"Deliver a new 400 volt 3CR12 SS orange powder coated IP65 rated outdoor Extraction fan control panel at the Cathedral Header Chamber complete with all circuit breakers, equipment, engraved labels and galvanized steel pedestal frame.","Sum",1]
["G3.7",null,"Deliver  seven  new 400 volt 3CR12 SS orange powder coated IP65 rated outdoor valve isolation  panels close to each of the actuators at the Cathedral Header Chamber complete with all circuit breakers, equipment, engraved labels and galvanized steel pedestal frames.","Sum",1]
["G3.8",null,"Deliver two  new 400 volt 3CR12 SS orange powder coated IP65 rated valve isolation  panels close to each actuator at the Engine Room no.4 valve isolation chamber complete with all circuit breakers, equipment, engraved labels and galvanized steel pedestal frame.","Sum",1]
["G3.9",null,"Deliver all power and control cabling complete with terminations","Sum",1]
["G3.10",null,"Deliver all earth cabling complete with terminations","Sum",1]
["G3.11",null,"Delivery of all earthing and bonding for all equipment and structures in accordance with SANS 10142-1","Sum",1]
["G3.12",null,"Delivery of all concrete cable markers complete with engraved name plates","Sum",1]
["G3.13",null,"Delivery of danger tape as per Rand Water requirements for  the cable excavations.","Sum",1]
["G3.14",null,"Delivery of sifted soil for the cable bed in the cable trench excavations.  ","Sum",1]
["G3.15",null,"Delivery of cable sealing system(no foam  or epoxy type systems shall be excepted)","Sum",1]
["G3.16",null,"Delivery of all  cable entry sleeves into and exiting the building ","Sum",1]
["G3.17",null,"Delivery of 110 mm PVC sleeves for road crossings complete with end caps and draw wire.","Sum",1]
["G3.18",null,"Deliver all SABS approved hot dipped galvanized cable rack/ ladders for a complete cable installation complete with cable rack/ ladder covers.","Sum",1]
["G3.19",null,"Delivery of all SABS approved galvanized conduits for the Cathedral Header and Engine Room 4 Chambers complete with all bends, joints, supports, termination boxes,etc.","Sum",1]
["G3.20",null,"Delivery of all socket outlets, switches and isolators forming part of this installation at the Cathedral Header and Engine Room 4 Chambers","Sum",1]
[]
[]
["Total Carried Forward ",{"$nulls":5},"R"]
["Total brought forward",{"$nulls":5},"R"]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No","Refers"]
[]
["G3.21",null,"Delivery of all light fittings forming part of this installation at the Cathedral Header and Engine Room 4 Chambers complete with all supports, mounting brackets and fixing systems complete with two spare fittings of each type of light fitting installed.","Sum",1]
["G3.22",null,"Deliver all 2.5mm² General Purpose insulated wire(phases + earth) for the installations forming part of  the Cathedral Header and Engine Room 4 Chambers","Sum",1]
["G3.23",null,"Deliver all 4mm² General Purpose insulated wire(phases + earth) for the installations forming part of  the Cathedral Header and Engine Room 4 Chambers","Sum",1]
["G3.24",null,"Deliver 24 Volt DC IP 65 adequately rated SABS approved  level control switches ","Sum",1]
["G3.25",null,"Deliver all engraved labels on all panels, kiosks, circuit breakers, equipment, outlets, isolators, light switches,etc.","Sum",1]
["G3.26",null,"Deliver all wire numbers and WKS cable labels.","Sum",1]
["G3.27",null,"Deliver all documentation as listed in the system specifications","Sum",1]
["G3.28",null,"Remove decommissioned small power and lighting installation and electrical equipment from site","Sum",1]
["G3.29",null,"Provide for Interface to Architectural, Mechanical, Automation and Civil/Structural requirements as part of the delivery process","Sum",1]
["H3.30",null,"Provision for supervision under this Bill item","Sum",1]
["G3.31",null,"Provide the details of any additional delivery  items not specifically mentioned, that might be required for a complete and working installation. If no details are provided below, any additional items required to complete the works shall be supplied, installed and commissioned at the contractors' cost. No further claims shall  be allowed on this item.","Sum",1]
[null,null,1]
[null,null,2]
[null,null,3]
[null,null,4]
[null,null,5]
[null,null,6]
[null,null,"Schedule H3 Carried Forward",{"$nulls":3},"R"]
[null,null,"BILL No.4"]
["G4",null,"INSTALLATION AND CONSTRUCTION"]
[null,"1 & 3","Modifications and Additions at Wash Water Power Supply Source"]
["G4.1",null,"Provision for the installation of an 125 amp 400 volt 36 kA circuit breaker with adjustable IDMT unit up to 1000 mA, in the emergency section of the 400 Volt MCC to supply new Kiosk no.1 complete with all cabling  and accessories for a complete installation.","Sum",1]
["G4.2",null,"Provision for the installation of a 63 amp 400 volt 36 kA breaker  with adjustable IDMT unit up to 1000 mA, in the emergency section of the 400 Volt MCC to supply new Kiosk no.2 complete with all accessories for a complete installation.","Sum",1]
[null,"1,4,5,6,7 & 8","Power Supply and Distribution"]
["G4.3",null,"Install a new 400 volt 3CR12 SS orange powder coated IP65 rated outdoor kiosk no.1 complete with all circuit breakers, equipment, engraved labels and galvanized steel pedestal frame.","Sum",1]
[]
[]
["Total Carried Forward ",{"$nulls":5},"R"]
["Total brought forward",{"$nulls":5},"R"]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No","Refers"]
[]
["G4.4",null,"Provision for a new 400 volt 3CR12 SS orange powder coated IP65 rated outdoor kiosk no.2 complete with all circuit breakers, equipment, engraved labels and galvanized steel pedestal frame. ","Sum",1]
["G4.5",null,"Install a new 400 volt 3CR12 SS orange powder coated IP65 rated outdoor small power and distribution board at the Cathedral Header Chamber complete with all circuit breakers, equipment, engraved labels and galvanized steel pedestal frame.","Sum",1]
["G4.6",null,"Provision for a new 400 volt 3CR12 SS orange powder coated IP65 rated outdoor small power and distribution board at Engine Room no.4 valve isolation chamber complete with all circuit breakers, equipment, engraved labels and galvanized steel pedestal frame.","Sum",1]
["G4.7",null,"Install two new 400 volt 3CR12 SS orange powder coated IP65 rated outdoor Sump pump control panels at the Cathedral Header Chamber complete with all circuit breakers, equipment, engraved labels and galvanized steel pedestal frame .(float switches covered elsewhere)","Sum",1]
["G4.8",null,"Install a new 400 volt 3CR12 SS orange powder coated IP65 rated outdoor Sump pump control panel at Engine Room no.4 valve isolation chamber complete with all circuit breakers, equipment, engraved labels and galvanized steel pedestal frame.(float switches covered elsewhere","Sum",1]
["G4.9",null,"Install a new 400 volt 3CR12 SS orange powder coated IP65 rated outdoor Extraction fan control panel at the Cathedral Header Chamber complete with all circuit breakers, equipment, engraved labels and galvanized steel pedestal frame.","Sum",1]
["G4.10",null,"Install seven  new 400 volt 3CR12 SS orange powder coated IP65 rated outdoor valve isolation  panels close to each of the actuators at the Cathedral Header Chamber complete with all circuit breakers, equipment, engraved labels and galvanized steel pedestal frames.","Sum",1]
["G4.11",null,"Install two  new 400 volt 3CR12 SS orange powder coated IP65 rated valve isolation  panels close to each actuator at the Engine Room no.4 valve isolation chamber complete with all circuit breakers, equipment, engraved labels and galvanized steel pedestal frame.","Sum",1]
[null,"1,10,11, 12,13 & 14","Power and Control Cabling Installation"]
["G4.12",null,"50mm² x 4 core Cu PVC SWAPVCPVC  power supply cable between 400 Volt MCC emergency section and Kiosk no.1 situated at the Cathedral Header Chamber ","m",150]
["G4.13",null,"25mm² x 4 core Cu PVC SWAPVCPVC  power supply cable between 400 Volt MCC emergency section and Kiosk no.2 situated at the Engine Room Valve Isolation Chamber","m",150]
["G4.14",null,"16mm² x 4 core Cu PVC SWAPVCPVC cable between kiosk no.1 and the SP&L distribution board at Cathedral Header Chamber","m",5]
["G4.15",null,"4mm² x 3 core Cu PVC SWAPVCPVC cable between the SP&L distribution board  and the first socket outlet at Cathedral Header Chamber","m",10]
[]
[]
["Total Carried Forward ",{"$nulls":5},"R"]
["Total brought forward",{"$nulls":5},"R"]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No","Refers"]
[]
["G4.16",null,"2.5mm² x 3 core Cu PVC SWAPVCPVC cable between the SP&L distribution board  and the first light switch at Cathedral Header Chamber","m",15]
["G4.17",null,"10mm² x 4 core Cu PVC SWAPVCPVC cable between kiosk no.1 and the two Sump pump control panels at Cathedral Header Chamber","m",50]
["G4.18",null,"4mm² x 4 core Cu PVC SWAPVCPVC cable between the two Sump pump control panels and each sump pump at Cathedral Header Chamber.","m",40]
["G4.19",null,"1.5mm² x 7 core Cu PVC SWAPVCPVC cable between the two Sump pump control panels and each sump pump level switches termination boxes at Cathedral Header Chamber.","m",40]
["G4.20",null,"4mm² x 4 core Cu PVC SWAPVCPVC cable between kiosk no.1 and the Extraction Fan control panel at Cathedral Header Chamber.","m",40]
["G4.21",null,"4mm² x 4 core Cu PVC SWAPVCPVC cable between the Extraction Fan control panel and the Extraction Fan at Cathedral Header Chamber.","m",5]
["G4.22",null,"10mm² x 4 core Cu PVC SWAPVCPVC cable between kiosk no.1 and each one of the seven Valve Isolation panels at the Cathedral Header actuators.","m",170]
["G4.23",null,"6mm² x 4 core Cu PVC SWAPVCPVC cable between each of the seven actuator valve isolation panels and each actuator at the Cathedral Header.","m",30]
["G4.24",null,"16mm² x 4 core Cu PVC SWAPVCPVC cable between kiosk no.2 and the SP&L distribution board at Engine Room 4 Isolation Chamber","m",5]
["G4.25",null,"2.5mm² x 3 core Cu PVC SWAPVCPVC cable between the SP&L distribution board  and the first light switch at Engine Room 4 Isolation Chamber ","m",15]
["G4.26",null,"10mm² x 4 core Cu PVC SWAPVCPVC cable between kiosk no.2 and the Sump pump control panel at Engine Room 4 Isolation Chamber","m",15]
["G4.27",null,"4mm² x 4 core Cu PVC SWAPVCPVC cable between the Sump pump control panel and the sump pump at Engine Room 4 Isolation Chamber.","m",40]
["G4.28",null,"1.5mm² x 7 core Cu PVC SWAPVCPVC cable between the Sump pump control panel and the sump pump level switches termination boxes at Engine Room 4 Isolation Chamber.","m",40]
["G4.29",null,"10mm² x 4 core Cu PVC SWAPVCPVC cable between kiosk no.2 and each one of the two Valve Isolation panels at the Engine Room 4 Isolation Chamber actuators.","m",50]
["G4.30",null,"6mm² x 4 core Cu PVC SWAPVCPVC cable between each of the two valve isolation panels and each actuator at the Engine Room 4 Isolation Chamber.","m",6]
[null,"1,10,11, 12,13 & 14","Cable Termination Installations"]
[null,null,"Includes SANS approved metal type glands, PVC shrouds, lugs and any other material required for a complete installation"]
["G4.31",null,"50mm² x 4 core Cu PVC SWAPVCPVC cable","No",2]
["G4.32",null,"25mm² x 4 core Cu PVC SWAPVCPVC cable","No",2]
["G4.33",null,"16mm² x 4 core Cu PVC SWAPVCPVC cable","No",4]
["G4.34",null,"10mm² x 4 core Cu PVC SWAPVCPVC cable","No",22]
["G4.35",null,"6mm² x 4 core Cu PVC SWAPVCPVC cable","No",18]
["G4.36",null,"4mm² x 3 core Cu PVC SWAPVCPVC cable","No",2]
["G4.37",null,"2.5mm² x 3 core Cu PVC SWAPVCPVC cable","No",4]
["G4.38",null,"1.5mm² x 7 core Cu PVC SWAPVCPVC cable","No",4]
[]
[]
["Total Carried Forward ",{"$nulls":5},"R"]
["Total brought forward",{"$nulls":5},"R"]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No","Refers"]
[]
[null,"1,10,11, 12,13 & 14","Earth Conductors "]
["G4.39",null,"25mm² Cu equivalent  Anti-theft type copper coated metal clad steel earth conductor for kiosk no.1","m",150]
["G4.40",null,"16mm² Cu equivalent  Anti-theft type copper coated metal clad steel earth conductor for kiosk no.2","m",150]
["G4.41",null,"6mm² black insulated copper earth conductor to run with power supply cabling for all other control panels and distribution boards","m",450]
["G4.42",null,"Earth conductors for all bonding and earthing requirements ","Sum",1]
[null,"1,10,11, 12,13 & 14","Terminations for Earth Conductors complete with SABS approved lugs and shrouds."]
["G4.43",null,"25mm² Cu equivalent  Anti-theft type copper coated metal clad steel earth conductor for kiosk no.1 ","No",2]
["G4.44",null,"16mm² Cu equivalent  Anti-theft type copper coated metal clad steel earth conductor for kiosk no.2 ","No",2]
["G4.45",null,"6mm² black insulated copper earth conductor for all other control panels and distribution boards ","No",32]
["G4.46",null,"Terminations for all Earth conductors for all bonding and earthing requirements ","Sum",1]
[null,"1,10,11, 12,13 & 14","Site Works for Cable Installation"]
["G4.47",null,"Install water, UV and corrosion resistant modular type cable sealing system at all cable entries into concrete chambers complete with core drilling where required(no resin or foam type allowed)","Sum",1]
["G4.48",null,"Excavation of cable trenching","Sum",1]
["G4.49",null,"Install Sifted soil to be utilized for PVC sleeve bedding inside cable trench excavation (100mm below cable and 150mm above cable)","Sum",1]
["G4.50",null,"Install SABS approved Danger tape 200mm above cable on entire length of excavation","Sum",1]
["G4.51",null,"Backfilling of cable trenching","Sum",1]
["G4.52",null,"Compaction of cable trenching","Sum",1]
["G4.53",null,"Install Cable route markers shall consist of concrete blocks with a concrete strength of at least 25 MPa, in the shape of truncated pyramid, approximately 300 mm high, 150 x 150 mm at the top and 250 x 250 mm at the bottom Aluminium plates shall be cast into the top of the blocks in such a manner that they cannot be pried loose. Power cable details and direction to be indicated on plate.","No",5]
["G4.54",null,"Install 110mm PVC sleeves for underground use to house the electrical cabling","m",24]
["G4.55",null,"Install 110mm PVC sleeve termination ends, joints, bends and end caps for electrical sleeves","Sum",1]
["G4.56",null,"Repair and reinstate all damaged surfaces affected by cable trench excavations","Sum",1]
["G4.57",null,"Install SABS approved hot dipped galvanized cable rack/ ladders for a complete cable installation complete with cable rack/ ladder covers.","Sum",1]
["G4.58",null,"Install SABS approved hot dipped galvanized cable rack/ ladder pre-manufactured joints, bends and supports for a complete cable installation complete with cable rack/ ladder covers and fixings.","Sum",1]
[]
[]
["Total Carried Forward ",{"$nulls":5},"R"]
["Total brought forward",{"$nulls":5},"R"]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No","Refers"]
[]
[null,"1 & 9","Conduits and Power Systems Installation"]
["G4.59",null,"25mm SABS approved surface mounted galvanized conduit for small power and lighting installations at the Cathedral Header Chamber.","Sum",1]
["G4.60",null,"25mm galvanized conduit loop in boxes, termination boxes, covers, couplings, bends, adaptors and supports for a complete installation at the Cathedral Header Chamber.","Sum",1]
["G4.61",null,"25mm SABS approved surface mounted galvanized conduit for small power and lighting installations at the Engine Room 4 Isolation Chamber.","Sum",1]
["G4.62",null,"25mm galvanized conduit loop in boxes, termination boxes, covers, couplings, bends, adaptors and supports for a complete installation at the Engine Room 4 Isolation Chamber.","Sum",1]
[null,"1 & 9","Socket Outlets, Switches and Isolators Installation"]
["G4.63",null,"230 volt 16 amp IP65 rated surface mounted socket outlet ","No",6]
["G4.64",null,"230 volt IP65 rated surface mounted single lever light switch ","No",2]
["G4.65",null,"400 volt 3pole 60 amp IP65 rated surface mounted isolator at sump pump ","No",3]
["G4.66",null,"400 volt 3pole 60 amp IP65 rated surface mounted isolator at extraction fan","No",1]
["G4.67",null,"400 Volt 32 Amp IP65 rated welding socket outlet complete with male socket","No",2]
[null,"1 & 7","Sump Pump Level Float Switches Installation"]
["G4.68",null,"24 Volt DC IP 65 adequately rated SABS approved  level control switches ","No",6]
[null,"1 & 9","General Purpose Insulated Conductors Installation"]
["G4.69",null,"2.5mm² General Purpose insulated wire(phases + earth)","Sum",1]
["G4.70",null,"4mm² General Purpose insulated wire(phases + earth)","Sum",1]
[null,"1 & 9","Luminair Installation"]
["G4.71",null,"SABS approved 230 Volt IP 65 rated 75 watt wide beam LED type flood light complete with mounting bracket. (level of 320 Lux to be achieved)","Sum",1]
["G4.72",null,"SABS approved 230 Volt IP 65 rated 75 watt wide beam LED type emergency  flood light complete with batteries and mounting bracket. (level of 320 Lux to be achieved)","Sum",1]
["G4.73",null,"SABS approved 230 Volt IP 65 rated 46 watt 1200mm LED type vapour proof light fitting (level of 320 Lux to be achieved)","Sum",1]
["G4.74",null,"SABS approved 230 Volt IP 65 rated 46 watt 1200mm LED type emergency vapour proof light fitting complete with batteries (level of 320 Lux to be achieved)","Sum",1]
["G4.75",null,"SABS approved 230 Volt IP 65 rated 7 watt green EXIT LED type  light fitting complete with internal batteries, mounting brackets and relevant pictogram ","Sum",1]
[null,"1 & 15","Miscellaneous Items"]
["G4.76",null,"Install Engraved labels for each isolator, socket outlet, light switch and distribution board ","Sum",1]
["G4.77",null,"Provide for all wire numbers and WKS cable labels.","Sum",1]
["G4.78",null,"Provision for the decommissioning of the existing SP&L installation in the Cathedral Header Chamber.","Sum",1]
[]
[]
["Total Carried Forward "]
["Total brought forward",{"$nulls":5},"R"]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No","Refers"]
[]
["G4.79",null,"Provision for the decommissioning of the existing electrical  installation in the Cathedral Header Chamber.","Sum",1]
["G4.80",null,"Provide for Interface to Architectural, Mechanical, Automation and Civil/Structural requirements under this bill item","Sum",1]
["G4.81",null,"Provision for supervision  under this Bill item","Sum",1]
["G4.82",null,"Provide the details of any additional installation and construction  items not specifically mentioned for all the areas forming part of this project, that might be required for a complete and working installation. If no details are provided below, any additional items required to complete the works shall be supplied, installed and commissioned at the contractors' cost. No further claims shall  be allowed on this item.","Sum",1]
[null,null,1]
[null,null,2]
[null,null,3]
[null,null,4]
[null,null,5]
[null,null,"Schedule H4 Carried Forward",{"$nulls":3},"R"]
[null,null,"BILL No.5"]
["G5",null,"PUTTING INTO SERVICE AND COMMISSIONING"]
[null,"1 & 3","Modifications and Additions at Wash Water Power Supply Source"]
["G5.1",null,"Putting into service and commissioning of the 125 amp 400 volt 36 kA circuit breaker with adjustable IDMT unit up to 1000 mA, in the emergency section of the 400 Volt MCC to supply new Kiosk no.1 complete with all cabling  and accessories for a complete installation.","Sum",1]
["G5.2",null,"Putting into service and commissioning of a 63 amp 400 volt 36 kA breaker  with adjustable IDMT unit up to 1000 mA, in the emergency section of the 400 Volt MCC to supply new Kiosk no.2 complete with all accessories for a complete installation.","Sum",1]
[null,"1,4,5,6,7,8,9,10 & 16","Power Supply and Distribution"]
["G5.3",null,"Putting into service and commissioning of Kiosk no.1 and Kiosk no.2 at the chambers  complete with cables, sleeves, cable supports,  etc.","Sum",1]
["G5.4",null,"Putting into service and commissioning of all small power and lighting distribution boards at the chambers  complete with cables, sleeves, cable supports,  etc.","Sum",1]
["G5.5",null,"Putting into service and commissioning of the extraction Fan distribution board at the Cathedral Header Chamber  complete with cables, sleeves, cable supports,  etc.","Sum",1]
["G5.6",null,"Putting into service and commissioning of all sump pump control panels at the chambers  complete with cables, sleeves, cable supports,  etc.","Sum",1]
["G5.7",null,"Putting into service and commissioning of all valve isolation panels at the chambers  complete with cables, sleeves, cable supports,  etc.","Sum",1]
["G5.8",null,"Putting into service and commissioning of all power, control, earthing and bonding cables complete with cable sealing systems. ","Sum",1]
["G5.9",null,"Putting into service and commissioning of all engraved labels on relevant equipment and outlets as well as all  WKS  type labeling on relevant equipment","Sum",1]
[]
[]
["Total Carried Forward ",{"$nulls":5},"R"]
["Total brought forward",{"$nulls":5},"R"]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No","Refers"]
[]
["G5.10",null,"Putting into service and commissioning of the complete small power and lighting installations complete with all distribution boards and issuing of an COC certificates","Sum",1]
[null,"1,2 & 16","Documentation"]
["G5.11",null,"Provision for all As Built and PR Eng. signed off drawings, schematics, site plans, GA's, etc. in hard and soft copy formats. ","Sum",1]
["G5.12",null,"Provision for all test reports complete with signed off FAT & SAT documentation for relevant equipment","Sum",1]
["G5.13",null,"Provision for a lux level test report complete with proof of calibrated test equipment.","Sum",1]
["G5.14",null,"Provision for all operation and maintenance manuals","Sum",1]
["G5.15",null,"Provision for all data sheets on equipment","Sum",1]
["G5.16",null,"Provision for all warrantees and guarantees on relevant equipment","Sum",1]
["G5.17",null,"Provision for 3 copies of electrical data books once draft copy is approved","Sum",1]
["G5.18",null,"Provide for supervision during the putting into service and commissioning process","Sum",1]
["G5.19",null,"Provide for interface with other disciplines during the  putting into service and commissioning process","Sum",1]
["G5.20",null,"Provide the details of any additional putting into service & commissioning related items not specifically mentioned, that might be required for a complete and working installation. If no details are provided below, any additional items required to complete the works shall be supplied, installed and commissioned at the contractors' cost. No further claims shall  be allowed on this item.","Sum",1]
[null,null,1]
[null,null,2]
[null,null,3]
[null,null,4]
[null,null,5]
[null,null,6]
[null,null,"Schedule H5 Carried Forward",{"$nulls":3},"R"]
[null,null,"Schedule Summary"]
[]
["No",null,"Description",{"$nulls":3},"Amount"]
["G1",null,"Detailed design"]
["G2",null,"Manufacture, supply and test"]
["G3",null,"Delivery of equipment"]
["G4",null,"Installation and construction"]
["G5",null,"Putting into service and commissioning"]
[]
[null,null,"Total Excluding VAT Schedule G Carried Forward to Summary Schedule",{"$nulls":3},{"v":0,"d":"R0.00"}]

{"sheet":"SCHEDULE H - Mechanical","index":9,"n_rows":94,"n_cols":7,"rows_kept":94,"merged":[[0,2,0,5],[1,2,1,4],[64,0,66,0],[64,1,66,1],[64,2,65,2],[93,0,94,5],[93,6,94,6],[96,0,96,6]],"flags":["formulas_cached_only"]}
[null,null,"CONSTRUCTION OF THE CATHEDRAL HEADER CHAMBER AT"]
[null,null,"VEREENIGING PUMPING STATION",{"$nulls":3},"SCHEDULE I: MECHANICAL"]
[]
["Item No.","Reference: RW01491-18 Doc Mech -01","Description","UNIT","Qty","Rate ","AMOUNT "]
["H1",null,"Design, supply, Manufacture and delivery"]
[]
["H1.1",2.1,"Mechanical Ventilation system "]
["H1.1.1",null,"Detail Design including calculation and development of drawings etc. for the mechanical ventilation system as typical shown on drawing RA-29162/02","Sum",1]
[]
["H1.2",2.2,"Sump Pump system"]
["H1.2.1",null,"Detail Design including calculation and development of drawings etc. for the sump pump system(s) as typical shown on drawing(s) RA-29162/02 and RA-29162/00","Sum",1]
[]
["H1.3","2.3.3","Valve Actuator Spindle & Sleeve"]
["H1.3.1",null,"Detail Design including calculation and development of drawings etc. for the Valve actuator extended spindle and sleeve complete with support and fittings etc.  as typical shown on drawing(s) RA-29162/01","Sum",1]
[]
["H1.4",null,"Manufacture, Supply , and delivery "]
[]
["H1.4.1",2.1,"Mechanical Ventilation system "]
["H1.4.1.1",null,"Mechanical ventilation system complete with fans, ducting, supports and fittings etc. as typical shown on drawing RA-29162/02 and RA-29162/00","Sum",1]
[]
["H1.4.2",null,"Sump Pump system"]
["H1.4.2.1","2.2.3","Sump pumps delivering 9 l/s @ 13m head  complete with piping, NRVs, flex connectors, valves and fittings etc. as typical shown on drawing RA-29162/02 and RA-29162/00","each",2]
[]
["H1.4.3",null,"Scour Valves"]
["H1.4.3.1",2.3,"DN 200mm with Test Pressure of 1500kPa scour valves.  As typical shown on drawing(s) RA-17924 ","each ",4]
[]
["H1.4.4",null,"Valve Actuator Spindle & Sleeve"]
["H1.4.4.1","\n2.4.3","Valve actuator extended spindle and sleeve complete with support and fittings etc.  as typical shown on drawing(s) RA-29162/01","Sum",1]
[]
["H1.5","2.4 & 2.5","Recondition & Repairs "]
[]
["H1.5.1",null,"Valves (Provided by Rand Water)"]
[null,null,"Collect, transport (to & fro Rand Water Site & Contractor site), and inspect and reconditioning & servicing  of valves complete with gearbox & actuator "]
["H1.5.1.1",null,"1600  dia mm ","each ",4]
["H1.5.1.2",null,"2500 dia  mm ","each ",5]
[]
["H1.5.2",2.4,"Access Steel Work "]
["H1.5.2.1",null,"Remove, transport and  Refurbish  access steel platforms, ladders , stanchions and fittings etc.  ","Sum",1]
[]
["H1.6",null,"Installation, commissioning and putting into service of Equipment  "]
[]
["H1.6.1",null,"Mechanical ventilation system complete with fans, ducting, supports and fittings etc. ","Sum",1]
[]
["H1.6.2",null,"Sump pumps delivering complete with piping, NRVs, flex connectors, valves and fittings etc. including scour valves ","Sum",1]
[]
["H1.6.3",null,"Access steel platforms, ladders , stanchions and fittings & etc.","Sum",1]
[]
["H1.7","Reference: RW01491-18 Doc Mech -01","Hand Over"]
[]
["H1.7.1",null,"Training of Rand Water Personnel","Sum",1]
[]
["H1.7.2",null,"Operation & Maintenance Manuals  (six copies)","Sum",1]
[]
["H1.7.3",null,"Maintenance during the defects & liability period.","Sum",1]
[]
["H1.7.4",null,"Compilation of As Built (record) drawings, close-out reports","Sum",1]
[]
["H1.7.5",null,"All other equipment /consumables/service  not stated above which are  required to complete and commission the Installation"]
[]
[]
[null,null,"Sub-section H1 Total",{"$nulls":3},0]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No","Refers"]
[]
["H2","Reference: RW01491-18 Doc Mech -01","ENGINE ROOM 4 VALVES"]
[]
[]
[]
["H2.1",null,"Removal, Transport and dliver at Central Depot  Of Existing Valves  ","Sum",1]
[]
["H2.2",2.6,"Manufacture, Test, Supply and delivey of  900mm diameter  flanged Rising Spindle Sluice valves, including dismantling couplings, gaskets and fittings. Flanged to A11791 5 000kPa Test Pressure complying to Rand Water specifications. RW /0310/AS 0460","No",5]
[]
["H2.3",2.6,"Manufacture, Test, Supply and delivey of  150mm diameter flanged non Rising spindle Sluice valves, including gaskets and fittimngs. Flanged to A11791 5000 kPa Test Pressure complying to Rand Water specifications. RW /0310/AS 0460","No",5]
[]
["H2.4",2.6,"Manufacture, Test, Supply and delivery of actuator, complete with gearbox, actuator and fittings etc. for  900mm diameter Sluice valve with TP  5 000kPa valve: ","No",5]
[]
["H2.5",2.7,"Manufacture, Test, Supply and delivery of  900mm diameter NRV  valve as per Rand Water Specifiction RW/0310/AS0460  delivery of a flanged non return valve, including dismantling couplings, gaskets and fittings. Flanged to A11791, 5 000kPa Test Pressure complying to Rand Water specifications.","No",5]
[]
["H2.2",null,"Installation, commissioning and putting into service  "]
["H2.2.1",null,"Installation, commissioning and putting into service of sluice valves complete  with  actuator, by pass valve/s , gaskets , fitttings bolts and nuts etc. ","Set ",5]
[]
["H2.2.2",null,"Installation, commissioning and putting into service of NRV complete  with gaskets , fitttings bolts and nuts etc. ","Set ",5]
[]
["H2.2.3",null,"Training of Rand Water Personnel","Sum",1]
[]
["H2.2.4",null,"Operation & Maintenance Manuals  (six copies)","Sum",1]
[]
["H2.2.5",null,"Maintenance during the defects & liability period.","Sum",1]
[]
["H2.2.6",null,"All other equipment /consumables/service  not stated above which are  required to complete and commission the Installation","Sum",1]
[]
[]
[null,null,"Sub-section H2 Total",{"$nulls":3},0]
["TOTAL SECTION H CARRIED FORWARD TO SUMMARY",{"$nulls":5},0]

{"sheet":"SCHEDULE I - PIPELINE","index":10,"n_rows":167,"n_cols":7,"rows_kept":167,"merged":[[0,2,0,5],[1,2,1,4],[55,0,55,2],[59,0,59,2],[116,0,116,2],[120,0,120,2],[166,0,166,2]],"flags":["formulas_cached_only"]}
[null,null,"CONSTRUCTION OF THE CATHEDRAL HEADER CHAMBER AT"]
[null,null,"VEREENIGING PUMPING STATION"]
[]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No","Refers"]
[null,null,"SANS 1200L"]
["I","SAM DOP 00001 TS","SECTION I:  VALVE CHAMBERS - VALVES AND PIPE SPECIALS"]
[]
["I1","TS 5.11","PIPE SPECIALS AND FITTINGS"]
[]
[null,null,"Manfacture and deliver of pipe fittings, complete as per Drawing: RA17924 rev 3 and R028765/100 incl alterations to existing pipework. Including supply of material, handling in accordance with specifications. Rate to include joining with flanges as required and making good of lining and coating. Flanges tobe in accordance to Rand Water Specification (Drawing A11791) including bolts, washers, nuts and gaskets."]
[]
["I1.1",null,"Item 1.1 & 1.6 - T-piece , 22mm x 2500mm OD by 12mm x 1600mm OD (two ends flanged) (pre-assemble items 1.1, 1.3 & 1.4 lined and coated)","No.",2]
[]
["I1.2",null,"Item 1.2 - T-piece, 22mm x 2500mm OD by 12mm x 1600mm OD (three ends flanged) (pre-assemable items 1.2 & 1.4 lined and coated)","No.",2]
[]
["I1.3",null,"Item 1.3 - Straight pipe, 10.97mm x 168.3mm OD  straight pipe (one end flanged)","No.",4]
[]
["I1.4",null,"Item 1.4 - Straight pipe, 12.7mm x 812mm OD straight pipe (one end flanged)","No.",4]
[]
["I1.5",null,"Item 1.5 - 16mm x 2500mm OD Wrapper plate,","No.",2]
[]
["I1.6",null,"Item 1.7 - Straight pipe, 12.7mm x 1600mm OD straight pipe (one end flanged)","No.",4]
[]
["I1.7",null,"Item 1.8 - 16mm x 1600mm OD Wrapper plate,","No.",4]
[]
["I1.8",null,"Item 1.9 - 6mm thick Compenstion plate,  shaped for 2528mm pipe","No.",4]
[]
["I1.9",null,"150mm x 150mm x 10mm rolled angle 2536mm dia ID fixed to existing concrete wall with 60No 16mm dia anchors. To provide pipe support.","No.",2]
[]
["I1.10",null,"150mm x 150mm x 10mm rolled angle 1632mm dia ID fixed to existing concrete wall with 38No 16mm dia anchors. To provide pipe support","No.",4]
[]
["I1.11",null,"Puddle flange to suite 2500mm pipe (Dwg No.: R028765/100) installed complete on existing pipe according to RA26448","No.",4]
[]
["I1.12",null,"DN 100mm dia, Grade X42 steel, 10mm thick, 150mm long stub fitted on the  2500mm pipe (Dwg No.: R028765/100) with blank flange for Chlorine Sampling","No.",4]
[]
["I2","TS 5.8","LINING AND COATING"]
[]
[null,null,"Completion of protective lining and coatng at joints. Supply material, and labour to execute the works"]
[]
["I2.1",null,"Remove existing coating for already manufactured specials","No.",4]
[]
["I2.2",null,"Apply coating as per specification","No.",4]
[]
["I2.3",null,"Internal lining - as per specification (solvent free) - 750 microns","No.",12]
[]
["I2.4",null,"External coating - as per specification (solvent free) - 2mm","No.",12]
[]
["I3","TS 5.16","HYDRO TESTING"]
[]
[null,null,"All pipes to be hydro tested before installation"]
[]
["I3.1",null,"Pipe Specials","No",8]
[]
[]
["Total Carried Forward "]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No","Refers"]
[]
["Total brought forward "]
[]
["I3.2",null,"ISOLATION OF WORKS"]
[]
["I3.2.1",null,"Supply, deliver and install and removal of isolating mechanism to existing header.","No.",2]
[]
["I3.2.2",null,"Supply and deliver (1700mm NB dia x 10mm thick blank flange) to isolate","No.",2]
[]
["I3.2.3",null,"Supply and deliver (2600mm NB dia x 10mm thick blank flange) to isolate","No.",2]
[]
["I3.2.4",null,"Isolation of existing header (insertion of spade (1700mm NB dia x 10mm thick blank flange) to isolate","No.",4]
[]
["I3.2.5",null,"Isolation of existing header (insertion of spade (2600mm NB dia x 10mm thick blank flange) to isolate","No",2]
[]
["I3.2.6",null,"Dewater of chamber and keeping the works dry during installation","Sum",1]
[]
["I3.2.7",null,"Other method of isolation (stipulated by the Contractor approved by the Engineer","No.",4]
[]
["I3.2.8",null,"Removal of existing pipe work","No.",8]
[]
["I3.2.9",null,"Removal of isolating mechanisms","No.",8]
[]
["I4","TS5.7","INSTALLATION OF T - PIECES AND WRAPPERS"]
[]
[null,null,"Installation of pipe fittings, complete as per Drawing: RA17924 rev 2 incl alterations to existing pipework. Rate to include joining as required and making good of lining and coating. Flanges to be in accordance to Rand Water Specification (Drawing A11791) including bolts, washers, nuts and gaskets."]
[]
["I4.1",null,"Item 1.1, 1.2, 1.6 - T-piece","No.",4]
[]
["I4.2",null,"Item 1.7 - Flanged pipe","No.",4]
[]
["I4.3",null,"2500mm dia  - Wrapper (internal)","No.",2]
[]
["I4.4",null,"2500mm dia  - Wrapper (external)","No.",2]
[]
["I4.5",null,"1600mm dia  - Wrapper (internal)","No.",4]
[]
["I4.6",null,"1600mm dia  - Wrapper (external)","No.",4]
[]
["I5","TS 5.15","TESTING OF WELDS TO 100% NDE"]
[]
["I5.1",null,"2500mm dia ","No.",4]
[]
["I5.2",null,"1600mm dia  ","No.",4]
[]
["I5.3",null,"Extra over on items ","No.",4]
[]
["I6","TS 5.12","VALVES TO BE SUPPLIED BY RW FREE OF CHARGE"]
[]
[null,null,"Collect from Vereeniging Pump Station transport to site, off load and install the following valves and fittings. Including the supply of bolts as required"]
[]
["I6.1",null,"2500mm dia Valve ","No.",5]
[]
["I6.2",null,"1600mm dia Valve ","No.",4]
[]
["I6.3",null,"200mm dia Valve","No.",4]
[]
[]
["Total Carried Forward "]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No","Refers"]
[]
["Total brought forward "]
[]
["I7","TS 5.13","Cathodic Protection - Insulating flanges "]
[]
[null,null,"Supply of flanges with gasket for cathodic insulating flanges for the following diameters, including installation, fittings, sleeves, tightening and setting of gasket rings, flange bolts, nuts and washers:"]
[]
["I7.1",null,"2500mm dia ","No.",10]
[]
["I7.2",null,"1600mm dia  ","No.",8]
[]
["I8",null,"All other Pipelines Equipment and actions not stated above which may be required to complete and commission the Installation (including risk mitigation and safety)","Prov Sum",500000,null,{"v":500000,"d":"500,000.00"}]
[]
["I8.1",null,"Contractors mark-up on above item","%"]
[]
["I9",null,"Condition Assesment as per Asset Manager requirements once pipeline is avaliable","Prov Sum",500000,null,{"v":500000,"d":"500,000.00"}]
[]
["I9.1",null,"Contractors mark-up on above item","%"]
[]
["I10",null,"Condition assessment of Chamber to mount the T-pieces","Prov Sum",100000,null,{"v":100000,"d":"100,000.00"}]
[]
["I10.1",null,"Contractors mark-up on above item","%"]
[]
["I11","TS 5.17","Standing Time","Days",55]
{"$rows_empty":23}
["Section I Carried Forward to Summary"]

{"sheet":"SCHEDULE J - SED","index":11,"n_rows":55,"n_cols":7,"rows_kept":55,"merged":[[0,2,0,5],[1,2,1,4],[1,7,2,7]],"flags":["formulas_cached_only"]}
[null,null,"CONSTRUCTION OF THE CATHEDRAL HEADER CHAMBER AT"]
[null,null,"VEREENIGING PUMPING STATION",{"$nulls":3},"SCHEDULE J - SED"]
[]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No","Refers"]
[]
["J",null,"SOCIO ECONOMIC DEVELOPMENT "]
[]
["J1",null,"SKILLS DEVELOPMENT PROGRAM"]
[]
["J1.1",null,"Accredited training programmes are targeted which will provide the beneficiaries with significant and recognized credit value in accordance with the National Qualification Framework (NQF). ","Sum",1]
[]
["J1.2",null,"Contractors mark-up on Items J1.1","%"]
[]
[]
["J2",null,"CORPORATE SOCIAL RESPONSIBILITY PROGRAM"]
[]
["J2.1",null,"Corproate Social Responsinislity programs aimed at improving the livelihood of the community","Sum",1]
[]
["J2.2",null,"Contractors mark-up on Items J2.1","%"]
[]
["J3",null,"COMMUNITY LIASON OFFICER"]
[]
["J3.1",null,"Community Liason Officer. A key component in aiding the realisation of the SED objectives is effective community liaison with all the relevant role-players, structures, civic organisations and the community at large.","Sum",1]
[]
["J3.2",null,"Contractors mark-up on Items J3.1","%"]
[]
["J4",null,"PARTICIPATION OF LOCAL ENTERPRISES"]
[]
["J4.1",null,"Work Allocated to Local Enterprises  (Inclusive of P&G's and SHEQ) (Minimum 5% of Project Value)","Sum",1]
[]
["J4.2",null,"Contractors mark-up on Items J4.1","%"]
[]
[]
["J5",null,"QUALITY CONTROL AND ASSURANCE "]
[]
["J5.1","8.4.3","Supervision for duration of construction including Quality Assurance as per TS 3.2 and TS2.33 including equipment factory acceptance tests","Sum",1]
[]
["J5.2",null,"Provision of Quality Control Plans ","Sum",1]
[]
["J5.3",null,"Provision of Welding, Coating and NDT inspection personel","Sum",1]
[]
["J5.4",null,"Maintenance of Testing equipments ( Calibration of Equipment ) ","Rate ",1]
[]
["J5.5","PS A 8.10","Quality control and all activities necessary to comply with all requirements of the specified quality control system as per PS 5 & TS2.32.","Sum",1]
[]
["J5.6",null,"Provision for Training of Quality control personel","Sum",1]
[]
["J5.7",null,"Maintenance of Testing and Inspection  documentation (Data Pack  Management)  and handing over to Rand Water prior to the commencement of the Defects Liability Period.","Sum ",1]
[]
[]
[]
[]
[]
[null,null,"Section J Carried Forward to Summary",{"$nulls":3},0]

{"sheet":"Summary","index":12,"n_rows":63,"n_cols":3,"rows_kept":63,"merged":[[19,5,19,7],[43,0,43,1],[47,0,47,1],[50,0,50,1],[53,0,53,1],[54,0,54,1],[55,0,55,1],[58,0,58,1],[60,0,60,2],[62,0,62,2]],"flags":["formulas_cached_only"]}
[]
[null,"SUMMARY"]
[]
["Section","Description","Amount"]
[]
[1,"SCHEDULE A: PRELIMINARY AND GENERAL"]
[]
[2,"SCHEDULE B: ENVIRONMENTAL"]
[]
[3,"SCHEDULE C: SHEQ"]
[]
[4,"SCHEDULE D: QUALITY"]
[]
[5,"SCHEDULE E: AUTOMATION"]
[]
[6,"SCHEDULE F: CIVIL"]
[]
[7,"SCHEDULE G: ELCTRICAL"]
[]
[8,"SCHEDULE H: MECHANICAL"]
[]
[9,"SCHEDULE I: PIPELINE"]
[]
[10,"SCHEDULE J: SED"]
{"$rows_empty":19}
["SUBTOTAL A ……………………………………..……………………………………………"]
[]
[]
[]
["CONTRACT PRICE ADJUSTMENT (Provisional Allowance)………………………….."]
[]
[]
["SUBTOTAL B ……………………...…..……………………………….……………………."]
[]
[]
["VALUE ADDED TAX"]
["Add 15% of Subtotal B ………..…….……………………..………...……..………………"]
["(Provisional sum based on current rate of VAT)"]
[]
[]
["TOTAL CARRIED TO FORM C1.1, FORM OF OFFER"]
[]
[]
[]
["SIGNED ON BEHALF OF TENDERER: ……………………………………………..……………………………………………."]