{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Spring Steel"],"not_rendered":{"defined_names":54},"read":"whole","date_system":"1900"}

{"sheet":"Spring Steel","index":0,"n_rows":94,"n_cols":36,"rows_kept":94,"merged":[[0,19,0,21],[0,22,0,24],[0,25,0,27],[0,28,0,30],[0,31,0,33],[0,34,0,35],[93,0,106,10]]}
[{"$nulls":19},"Year 1",null,null,"Year 2",null,null,"Year  3",null,null,"Year 4",null,null,"Year 5",null,null,"5 Year Totals"]
["Executive","ITEM NUMBER","ITEM DESCRIPTION","R/Y","Long text","Search1","UOM","Not steel item?","Spec","Grouping","Grade","Type","Seifsa","YEAR 1\n2025/26","YEAR 2\n2026/27","YEAR 3\n2027/28","YEAR 4\n2028/29","YEAR 5\n2029/30","TOTAL","Item Price Excl VAT","Total Excl VAT","Total Including 15% VAT","Item Price Excl VAT","Total Excl VAT","Total Including 15% VAT","Item Price Excl VAT","Total Excl VAT","Total Including 15% VAT","Item Price Excl VAT","Total Excl VAT","Total Including 15% VAT","Item Price Excl VAT","Total Excl VAT","Total Including 15% VAT","Total Excl VAT","Total Including 15% VAT"]
["Manufacturing","311201767","PLATE METAL;6 MM,WD:1.5 M,LG:2.5 M,STL",null,"PLATE, METALLIC; THICKNESS: 6 MM, WIDTH: 1.5 M, LENGTH: 2.5 M, PLATE MATERIAL: STEEL, MATERIAL GRADE: 3CR12 HRA; STEEL 6X1500X2500 SPEC. 3CR12 HRA","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,5,5,5,5,5,{"$f":"N3+O3+P3+Q3+R3","v":25},null,{"$f":"+T3*N3","v":0},{"$f":"U3*1.15","v":0},{"$f":"T3*1.06","v":0},{"$f":"(W3*O3)","v":0},{"$f":"X3*1.15","v":0},{"$f":"W3*1.06","v":0},{"$f":"(+Z3)*P3","v":0},{"$f":"AA3*1.15","v":0},{"$f":"Z3*1.06","v":0},{"$f":"(AC3)*Q3","v":0},{"$f":"AD3*1.15","v":0},{"$f":"AC3*1.06","v":0},{"$f":"(+AF3)*R3","v":0},{"$f":"AG3*1.15","v":0},{"$f":"AG3+AD3+AA3+X3+U3","v":0},{"$f":"AI3*1.15","v":0}]
["Manufacturing","611000270","PLATE METAL;4 MM,1565 MM,3282 MM",null,"PLATE, METALLIC; THICKNESS: 4 MM, WIDTH: 1565 MM, LENGTH: 3282 MM, MATERIAL GRADE: EN10088 3CR12; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED; FOR WAGON SIDE/BOTTOM; CCL","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,13,13,13,13,13,{"$f":"N4+O4+P4+Q4+R4","v":65},null,{"$f":"+T4*N4","v":0},{"$f":"U4*1.15","v":0},{"$f":"T4*1.06","v":0},{"$f":"(W4*O4)","v":0},{"$f":"X4*1.15","v":0},{"$f":"W4*1.06","v":0},{"$f":"(+Z4)*P4","v":0},{"$f":"AA4*1.15","v":0},{"$f":"Z4*1.06","v":0},{"$f":"(AC4)*Q4","v":0},{"$f":"AD4*1.15","v":0},{"$f":"AC4*1.06","v":0},{"$f":"(+AF4)*R4","v":0},{"$f":"AG4*1.15","v":0},{"$f":"AG4+AD4+AA4+X4+U4","v":0},{"$f":"AI4*1.15","v":0}]
["Manufacturing","511420113","PLATE METAL;4 MM,1200 MM,2500 MM",null,"PLATE, METALLIC; THICKNESS: 4 MM, WIDTH: 1200 MM, LENGTH: 2500 MM, MATERIAL GRADE: EN10088 3CR12; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED. HRA SURFACE CONDITION","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,41,41,41,41,41,205,null,{"$f":"+T5*N5","v":0},0,{"$f":"T5*1.06","v":0},{"$f":"(W5*O5)","v":0},0,{"$f":"W5*1.06","v":0},{"$f":"(+Z5)*P5","v":0},0,0,{"$f":"(AC5)*Q5","v":0},0,{"$f":"AC5*1.06","v":0},{"$f":"(+AF5)*R5","v":0},0,{"$f":"AG5+AD5+AA5+X5+U5","v":0},0]
["Project Wagons 1000","511420113","PLATE METAL;4 MM,1200 MM,2500 MM",null,"PLATE, METALLIC; THICKNESS: 4 MM, WIDTH: 1200 MM, LENGTH: 2500 MM, MATERIAL GRADE: EN10088 3CR12; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED. HRA SURFACE CONDITION","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,4,4,{"$nulls":3},8,null,{"$f":"+T6*N6","v":0},0,{"$f":"T6*1.06","v":0},{"$f":"(W6*O6)","v":0},0,{"$f":"W6*1.06","v":0},{"$f":"(+Z6)*P6","v":0},0,0,{"$f":"(AC6)*Q6","v":0},0,{"$f":"AC6*1.06","v":0},{"$f":"(+AF6)*R6","v":0},0,{"$f":"AG6+AD6+AA6+X6+U6","v":0},0]
["Manufacturing","014000884","SHEET METAL;3CR12 NO 2B FINISH,2.5,2.5 M",null,"SHEET, METALLIC; MATERIAL GRADE: 3CR12 NO 2B FINISH, THICKNESS: 2.5, WIDTH: 1.25 M, LENGTH: 2.5 M","SHEET","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,36,36,36,36,36,180,null,{"$f":"+T7*N7","v":0},0,{"$f":"T7*1.06","v":0},{"$f":"(W7*O7)","v":0},0,{"$f":"W7*1.06","v":0},{"$f":"(+Z7)*P7","v":0},0,0,{"$f":"(AC7)*Q7","v":0},0,{"$f":"AC7*1.06","v":0},{"$f":"(+AF7)*R7","v":0},0,{"$f":"AG7+AD7+AA7+X7+U7","v":0},0]
["Manufacturing","077770193","PIPE METAL;SMLS,PIPE SZ:OD 60.3 MM",null,"PIPE, METALLIC; TYPE: SEAMLESS, PIPE SIZE: OD 60.3 MM, LENGTH: 6 M, WALL THICKNESS: 3.91 MM, PIPE MATERIAL: STEEL ASTM 106, SCHEDULE: 40; MASS:- 5.43KG/M; GRADE:B","PIPE,","M",null,"ASTM A106 ","SST & 3CR12","Stainless Steel","Pipe & Tube",null,1,1,1,1,1,5,null,{"$f":"+T8*N8","v":0},0,{"$f":"T8*1.06","v":0},{"$f":"(W8*O8)","v":0},0,{"$f":"W8*1.06","v":0},{"$f":"(+Z8)*P8","v":0},0,0,{"$f":"(AC8)*Q8","v":0},0,{"$f":"AC8*1.06","v":0},{"$f":"(+AF8)*R8","v":0},0,{"$f":"AG8+AD8+AA8+X8+U8","v":0},0]
["Manufacturing","011665972","PLATE METAL;6 MM,1200 MM,3150 MM",null,"PLATE, METALLIC; THICKNESS: 6 MM, WIDTH: 1200 MM, LENGTH: 3150 MM, MATERIAL GRADE: EN 100088 3CR12; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,59,37,61,78,45,280,null,{"$f":"+T9*N9","v":0},0,{"$f":"T9*1.06","v":0},{"$f":"(W9*O9)","v":0},0,{"$f":"W9*1.06","v":0},{"$f":"(+Z9)*P9","v":0},0,0,{"$f":"(AC9)*Q9","v":0},0,{"$f":"AC9*1.06","v":0},{"$f":"(+AF9)*R9","v":0},0,{"$f":"AG9+AD9+AA9+X9+U9","v":0},0]
["Manufacturing","911500580","PLATE METAL;5 MM,WD:1.97 M,LG:4.665 M",null,"PLATE, METALLIC; THICKNESS: 5 MM, WIDTH: 1.97 M, LENGTH: 4.665 M, PLATE MATERIAL: STEEL, MATERIAL GRADE: 3CR12 FOR ALT REFER TO DRG PEW029C0031","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,145,97,171,225,158,796,null,{"$f":"+T10*N10","v":0},0,{"$f":"T10*1.06","v":0},{"$f":"(W10*O10)","v":0},0,{"$f":"W10*1.06","v":0},{"$f":"(+Z10)*P10","v":0},0,0,{"$f":"(AC10)*Q10","v":0},0,{"$f":"AC10*1.06","v":0},{"$f":"(+AF10)*R10","v":0},0,{"$f":"AG10+AD10+AA10+X10+U10","v":0},0]
["Manufacturing","368201782PREC","PLATE;SIDE,SS GR 3CR12",null,"PLATE; TYPE: SIDE, MATERIAL: STAINLESS STEEL GRADE 3CR12, DIMENSIONS: WD 498 MM X LG 2.28 M X THK 4 MM; PRC/CUT CAD; TOLERANCE WILL  BE (0+2)MM SQUARENESS AND (-1+1)MM ON LENGHT AND WIDTH","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,13,20,8,7,20,68,null,{"$f":"+T11*N11","v":0},0,{"$f":"T11*1.06","v":0},{"$f":"(W11*O11)","v":0},0,{"$f":"W11*1.06","v":0},{"$f":"(+Z11)*P11","v":0},0,0,{"$f":"(AC11)*Q11","v":0},0,{"$f":"AC11*1.06","v":0},{"$f":"(+AF11)*R11","v":0},0,{"$f":"AG11+AD11+AA11+X11+U11","v":0},0]
["Manufacturing","013001285","PIPE METAL;SEAMLESS,PIPE SZ:20 MM,LG:6 M",null,"PIPE, METALLIC; TYPE: SEAMLESS, PIPE SIZE: 20 MM, LENGTH: 6 M, WALL THICKNESS: 2.87 MM, PIPE MATERIAL: STEEL, MATERIAL GRADE: ASTM A106 B, SURFACE TREATMENT: PLAIN, END CONNECTION TYPE: STANDARD, SCHEDULE: 40, COLOR: BLACK","PIPE,","M",null,"ASTM A106","SST & 3CR12","Stainless Steel","Pipe & Tube",null,10,10,23,33,34,110,null,{"$f":"+T12*N12","v":0},0,{"$f":"T12*1.06","v":0},{"$f":"(W12*O12)","v":0},0,{"$f":"W12*1.06","v":0},{"$f":"(+Z12)*P12","v":0},0,0,{"$f":"(AC12)*Q12","v":0},0,{"$f":"AC12*1.06","v":0},{"$f":"(+AF12)*R12","v":0},0,{"$f":"AG12+AD12+AA12+X12+U12","v":0},0]
["Manufacturing","368201781PREC","PLATE METAL;SIDE,4 MM,WD:1.51 M,STL",null,"PLATE, METALLIC; TYPE: SIDE, THICKNESS: 4 MM, WIDTH: 1.51 M, LENGTH: 2.436 M, PLATE MATERIAL: STEEL, MATERIAL GRADE: 3CR12; PRC/CUT  CAD TOLERANCE WILL BE (0+2) MM SQUARENESS AND (-1+1) MM ON LENGTH AND WIDTH","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,3,4,2,2,5,16,null,{"$f":"+T13*N13","v":0},0,{"$f":"T13*1.06","v":0},{"$f":"(W13*O13)","v":0},0,{"$f":"W13*1.06","v":0},{"$f":"(+Z13)*P13","v":0},0,0,{"$f":"(AC13)*Q13","v":0},0,{"$f":"AC13*1.06","v":0},{"$f":"(+AF13)*R13","v":0},0,{"$f":"AG13+AD13+AA13+X13+U13","v":0},0]
["Manufacturing","611000279","PLATE METAL;TRIM,6 MM,WD:716 MM,STL",null,"PLATE, METALLIC; TYPE: TRIMMED, THICKNESS: 6 MM, WIDTH: 716 MM, LENGTH: 1.772 M, PLATE MATERIAL: STEEL, MATERIAL GRADE: 3CR12; PLEA SE NOTE: THE FOLLOWING L = 1772 +0 - 2MM W = 716 +0 - 2MM SQUARE = +-0 + 2MM","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,50,50,50,50,50,250,null,{"$f":"+T14*N14","v":0},0,{"$f":"T14*1.06","v":0},{"$f":"(W14*O14)","v":0},0,{"$f":"W14*1.06","v":0},{"$f":"(+Z14)*P14","v":0},0,0,{"$f":"(AC14)*Q14","v":0},0,{"$f":"AC14*1.06","v":0},{"$f":"(+AF14)*R14","v":0},0,{"$f":"AG14+AD14+AA14+X14+U14","v":0},0]
["Manufacturing","611000255","PLATE METAL;4 MM,1290 MM,2643 MM",null,"PLATE, METALLIC; THICKNESS: 4 MM, WIDTH: 1290 MM, LENGTH: 2643 MM, MATERIAL GRADE: EN10088 3CR12; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED. TOLERANCE OF LENGTH + WIDTH TO BE  +0 -2 TOLE","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,8,8,8,8,8,40,null,{"$f":"+T15*N15","v":0},0,{"$f":"T15*1.06","v":0},{"$f":"(W15*O15)","v":0},0,{"$f":"W15*1.06","v":0},{"$f":"(+Z15)*P15","v":0},0,0,{"$f":"(AC15)*Q15","v":0},0,{"$f":"AC15*1.06","v":0},{"$f":"(+AF15)*R15","v":0},0,{"$f":"AG15+AD15+AA15+X15+U15","v":0},0]
["Manufacturing","611000256","PLATE METAL;4 MM,1565 MM,1705 MM",null,"PLATE, METALLIC; THICKNESS: 4 MM, WIDTH: 1565 MM, LENGTH: 1705 MM, MATERIAL GRADE: EN10088 3CR12; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED. FABRICATION METHOD: HOT ROLLED","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,5,5,5,5,5,25,null,{"$f":"+T16*N16","v":0},0,{"$f":"T16*1.06","v":0},{"$f":"(W16*O16)","v":0},0,{"$f":"W16*1.06","v":0},{"$f":"(+Z16)*P16","v":0},0,0,{"$f":"(AC16)*Q16","v":0},0,{"$f":"AC16*1.06","v":0},{"$f":"(+AF16)*R16","v":0},0,{"$f":"AG16+AD16+AA16+X16+U16","v":0},0]
["Manufacturing","511420112","PLATE METAL;4 MM,1300 MM,2200 MM",null,"PLATE, METALLIC; THICKNESS: 4 MM, WIDTH: 1300 MM, LENGTH: 2200 MM, MATERIAL GRADE: EN10088 3CR12; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED. FABRICATION METHOD: HOT ROLLED. ZINC PLATED S","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,903,903,903,903,903,4515,null,{"$f":"+T17*N17","v":0},0,{"$f":"T17*1.06","v":0},{"$f":"(W17*O17)","v":0},0,{"$f":"W17*1.06","v":0},{"$f":"(+Z17)*P17","v":0},0,0,{"$f":"(AC17)*Q17","v":0},0,{"$f":"AC17*1.06","v":0},{"$f":"(+AF17)*R17","v":0},0,{"$f":"AG17+AD17+AA17+X17+U17","v":0},0]
["Manufacturing","914500232","PLATE METAL;4 MM,1100 MM,2200 MM",null,"PLATE, METALLIC; THICKNESS: 4 MM, WIDTH: 1100 MM, LENGTH: 2200 MM, MATERIAL GRADE: EN 10088 3CR12; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. ZINC PLATED STEEL FABRICATIO N METHOD: HOT ROLLED","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,54,54,54,54,54,270,null,{"$f":"+T18*N18","v":0},0,{"$f":"T18*1.06","v":0},{"$f":"(W18*O18)","v":0},0,{"$f":"W18*1.06","v":0},{"$f":"(+Z18)*P18","v":0},0,0,{"$f":"(AC18)*Q18","v":0},0,{"$f":"AC18*1.06","v":0},{"$f":"(+AF18)*R18","v":0},0,{"$f":"AG18+AD18+AA18+X18+U18","v":0},0]
["Project Wagons 1000","511420112","PLATE METAL;4 MM,1300 MM,2200 MM",null,"PLATE, METALLIC; THICKNESS: 4 MM, WIDTH: 1300 MM, LENGTH: 2200 MM, MATERIAL GRADE: EN10088 3CR12; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED. FABRICATION METHOD: HOT ROLLED. ZINC PLATED S","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,4948,4948,{"$nulls":3},9896,null,{"$f":"+T19*N19","v":0},0,{"$f":"T19*1.06","v":0},{"$f":"(W19*O19)","v":0},0,{"$f":"W19*1.06","v":0},{"$f":"(+Z19)*P19","v":0},0,0,{"$f":"(AC19)*Q19","v":0},0,{"$f":"AC19*1.06","v":0},{"$f":"(+AF19)*R19","v":0},0,{"$f":"AG19+AD19+AA19+X19+U19","v":0},0]
["Project Wagons 1000","914500232","PLATE METAL;4 MM,1100 MM,2200 MM",null,"PLATE, METALLIC; THICKNESS: 4 MM, WIDTH: 1100 MM, LENGTH: 2200 MM, MATERIAL GRADE: EN 10088 3CR12; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. ZINC PLATED STEEL FABRICATIO N METHOD: HOT ROLLED","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,6017,6017,{"$nulls":3},12034,null,{"$f":"+T20*N20","v":0},0,{"$f":"T20*1.06","v":0},{"$f":"(W20*O20)","v":0},0,{"$f":"W20*1.06","v":0},{"$f":"(+Z20)*P20","v":0},0,0,{"$f":"(AC20)*Q20","v":0},0,{"$f":"AC20*1.06","v":0},{"$f":"(+AF20)*R20","v":0},0,{"$f":"AG20+AD20+AA20+X20+U20","v":0},0]
["Manufacturing","611000274","PLATE METAL;8 MM,1565 MM,3860 MM",null,"PLATE, METALLIC; THICKNESS: 8 MM, WIDTH: 1565 MM, LENGTH: 3860 MM, MATERIAL GRADE: EN10088 3CR12; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED. FABRICATION METHOD: HOT ROLLED; MIN PROOF STR","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,5,5,5,5,5,25,null,{"$f":"+T21*N21","v":0},0,{"$f":"T21*1.06","v":0},{"$f":"(W21*O21)","v":0},0,{"$f":"W21*1.06","v":0},{"$f":"(+Z21)*P21","v":0},0,0,{"$f":"(AC21)*Q21","v":0},0,{"$f":"AC21*1.06","v":0},{"$f":"(+AF21)*R21","v":0},0,{"$f":"AG21+AD21+AA21+X21+U21","v":0},0]
["Manufacturing","611000248","PLATE METAL;6 MM,1565 MM,2170 MM,STL",null,"PLATE, METALLIC; THICKNESS: 6 MM, WIDTH: 1565 MM, LENGTH: 2170 MM, PLATE MATERIAL: STEEL, MATERIAL GRADE: EN 10088 3CR12, FABRICATION METHOD: HOT ROLLED; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFAC","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,10,10,10,10,10,50,null,{"$f":"+T22*N22","v":0},0,{"$f":"T22*1.06","v":0},{"$f":"(W22*O22)","v":0},0,{"$f":"W22*1.06","v":0},{"$f":"(+Z22)*P22","v":0},0,0,{"$f":"(AC22)*Q22","v":0},0,{"$f":"AC22*1.06","v":0},{"$f":"(+AF22)*R22","v":0},0,{"$f":"AG22+AD22+AA22+X22+U22","v":0},0]
["Manufacturing","914500581","PLATE METAL;6 MM,1565 MM,4100 MM",null,"PLATE, METALLIC; THICKNESS: 6 MM, WIDTH: 1565 MM, LENGTH: 4100 MM, MATERIAL GRADE: EN 10088 3CR12; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED. LENGTH; WIDTH UNTRIMMED. GRADE: 3CR12 (HRA).","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,113,69,115,147,86,530,null,{"$f":"+T23*N23","v":0},0,{"$f":"T23*1.06","v":0},{"$f":"(W23*O23)","v":0},0,{"$f":"W23*1.06","v":0},{"$f":"(+Z23)*P23","v":0},0,0,{"$f":"(AC23)*Q23","v":0},0,{"$f":"AC23*1.06","v":0},{"$f":"(+AF23)*R23","v":0},0,{"$f":"AG23+AD23+AA23+X23+U23","v":0},0]
["Project Wagons 1000","914500581","PLATE METAL;6 MM,1565 MM,4100 MM",null,"PLATE, METALLIC; THICKNESS: 6 MM, WIDTH: 1565 MM, LENGTH: 4100 MM, MATERIAL GRADE: EN 10088 3CR12; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED. LENGTH; WIDTH UNTRIMMED. GRADE: 3CR12 (HRA).","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,1002,1002,{"$nulls":3},2004,null,{"$f":"+T24*N24","v":0},0,{"$f":"T24*1.06","v":0},{"$f":"(W24*O24)","v":0},0,{"$f":"W24*1.06","v":0},{"$f":"(+Z24)*P24","v":0},0,0,{"$f":"(AC24)*Q24","v":0},0,{"$f":"AC24*1.06","v":0},{"$f":"(+AF24)*R24","v":0},0,{"$f":"AG24+AD24+AA24+X24+U24","v":0},0]
["Manufacturing","311200230","PLATE STEEL  6x1200x2800 HRA BL    3CR12",null,"PLATE STEEL (3CR12) 6x1200x2800 HRA BL SPEC. 3CR12 HRA BLACK","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,316,271,329,34,35,985,null,{"$f":"+T25*N25","v":0},0,{"$f":"T25*1.06","v":0},{"$f":"(W25*O25)","v":0},0,{"$f":"W25*1.06","v":0},{"$f":"(+Z25)*P25","v":0},0,0,{"$f":"(AC25)*Q25","v":0},0,{"$f":"AC25*1.06","v":0},{"$f":"(+AF25)*R25","v":0},0,{"$f":"AG25+AD25+AA25+X25+U25","v":0},0]
["Manufacturing","011670463","PLATE METAL;6 MM,1100 MM,3000 MM",null,"PLATE, METALLIC; THICKNESS: 6 MM, WIDTH: 1100 MM, LENGTH: 3000 MM, MATERIAL GRADE: EN 10088 3CR12; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED.","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,3,3,7,9,10,32,null,{"$f":"+T26*N26","v":0},0,{"$f":"T26*1.06","v":0},{"$f":"(W26*O26)","v":0},0,{"$f":"W26*1.06","v":0},{"$f":"(+Z26)*P26","v":0},0,0,{"$f":"(AC26)*Q26","v":0},0,{"$f":"AC26*1.06","v":0},{"$f":"(+AF26)*R26","v":0},0,{"$f":"AG26+AD26+AA26+X26+U26","v":0},0]
["Project Wagons 1000","011670463","PLATE METAL;6 MM,1100 MM,3000 MM",null,"PLATE, METALLIC; THICKNESS: 6 MM, WIDTH: 1100 MM, LENGTH: 3000 MM, MATERIAL GRADE: EN 10088 3CR12; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED.","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,144,144,{"$nulls":3},288,null,{"$f":"+T27*N27","v":0},0,{"$f":"T27*1.06","v":0},{"$f":"(W27*O27)","v":0},0,{"$f":"W27*1.06","v":0},{"$f":"(+Z27)*P27","v":0},0,0,{"$f":"(AC27)*Q27","v":0},0,{"$f":"AC27*1.06","v":0},{"$f":"(+AF27)*R27","v":0},0,{"$f":"AG27+AD27+AA27+X27+U27","v":0},0]
["Manufacturing","311030323","SHEET METAL;STL,3 MM,1250 MM,2500 MM",null,"SHEET, METALLIC; MATERIAL GRADE: NEW: EN 10088 3CR12, OLD GRADE 3CR12, MATERIAL: STEEL, THICKNESS: 3 MM, WIDTH: 1250 MM, LENGTH: 2500 MM; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED. EN 10","SHEET","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,46,67,38,37,77,265,null,{"$f":"+T28*N28","v":0},0,{"$f":"T28*1.06","v":0},{"$f":"(W28*O28)","v":0},0,{"$f":"W28*1.06","v":0},{"$f":"(+Z28)*P28","v":0},0,0,{"$f":"(AC28)*Q28","v":0},0,{"$f":"AC28*1.06","v":0},{"$f":"(+AF28)*R28","v":0},0,{"$f":"AG28+AD28+AA28+X28+U28","v":0},0]
["Manufacturing","914500231","PLATE METAL;4 MM,25.4 MM,3020 MM",null,"PLATE, METALLIC; THICKNESS: 4 MM, WIDTH:   25.4MM LENGTH: 3020 MM, MATERIAL GRADE: EN 10088 3CR12; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. ZINC PLATED STEEL. FABRICATION METHOD: HOT ROLLED","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,21,21,21,21,21,105,null,{"$f":"+T29*N29","v":0},0,{"$f":"T29*1.06","v":0},{"$f":"(W29*O29)","v":0},0,{"$f":"W29*1.06","v":0},{"$f":"(+Z29)*P29","v":0},0,0,{"$f":"(AC29)*Q29","v":0},0,{"$f":"AC29*1.06","v":0},{"$f":"(+AF29)*R29","v":0},0,{"$f":"AG29+AD29+AA29+X29+U29","v":0},0]
["Project Wagons 1000","914500231","PLATE METAL;4 MM,25.4 MM,3020 MM",null,"PLATE, METALLIC; THICKNESS: 4 MM, WIDTH:   25.4MM LENGTH: 3020 MM, MATERIAL GRADE: EN 10088 3CR12; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. ZINC PLATED STEEL. FABRICATION METHOD: HOT ROLLED","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,1000,1000,{"$nulls":3},2000,null,{"$f":"+T30*N30","v":0},0,{"$f":"T30*1.06","v":0},{"$f":"(W30*O30)","v":0},0,{"$f":"W30*1.06","v":0},{"$f":"(+Z30)*P30","v":0},0,0,{"$f":"(AC30)*Q30","v":0},0,{"$f":"AC30*1.06","v":0},{"$f":"(+AF30)*R30","v":0},0,{"$f":"AG30+AD30+AA30+X30+U30","v":0},0]
["Manufacturing","914500210","PLATE METAL;8 MM,1500 MM,3870 MM",null,"PLATE, METALLIC; THICKNESS: 8 MM, WIDTH: 1500 MM, LENGTH: 3870 MM, MATERIAL GRADE: EN 10088 3CR12; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED. FABRICATION METHOD: HOT ROLLED","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,15,15,15,15,15,75,null,{"$f":"+T31*N31","v":0},0,{"$f":"T31*1.06","v":0},{"$f":"(W31*O31)","v":0},0,{"$f":"W31*1.06","v":0},{"$f":"(+Z31)*P31","v":0},0,0,{"$f":"(AC31)*Q31","v":0},0,{"$f":"AC31*1.06","v":0},{"$f":"(+AF31)*R31","v":0},0,{"$f":"AG31+AD31+AA31+X31+U31","v":0},0]
["Project Wagons 1000","914500210","PLATE METAL;8 MM,1500 MM,3870 MM",null,"PLATE, METALLIC; THICKNESS: 8 MM, WIDTH: 1500 MM, LENGTH: 3870 MM, MATERIAL GRADE: EN 10088 3CR12; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED. FABRICATION METHOD: HOT ROLLED","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,392,392,{"$nulls":3},784,null,{"$f":"+T32*N32","v":0},0,{"$f":"T32*1.06","v":0},{"$f":"(W32*O32)","v":0},0,{"$f":"W32*1.06","v":0},{"$f":"(+Z32)*P32","v":0},0,0,{"$f":"(AC32)*Q32","v":0},0,{"$f":"AC32*1.06","v":0},{"$f":"(+AF32)*R32","v":0},0,{"$f":"AG32+AD32+AA32+X32+U32","v":0},0]
["Manufacturing","914500562","PLATE METAL;4 MM,1500 MM,2170 MM",null,"PLATE, METALLIC; THICKNESS: 4 MM, WIDTH: 1500 MM, LENGTH: 2170 MM, MATERIAL GRADE: EN 10088 3CR12; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED. ZINC PLATED STEEL. FABRICATION  METHOD: HOT","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,395,395,395,395,395,1975,null,{"$f":"+T33*N33","v":0},0,{"$f":"T33*1.06","v":0},{"$f":"(W33*O33)","v":0},0,{"$f":"W33*1.06","v":0},{"$f":"(+Z33)*P33","v":0},0,0,{"$f":"(AC33)*Q33","v":0},0,{"$f":"AC33*1.06","v":0},{"$f":"(+AF33)*R33","v":0},0,{"$f":"AG33+AD33+AA33+X33+U33","v":0},0]
["Project Wagons 1000","914500562","PLATE METAL;4 MM,1500 MM,2170 MM",null,"PLATE, METALLIC; THICKNESS: 4 MM, WIDTH: 1500 MM, LENGTH: 2170 MM, MATERIAL GRADE: EN 10088 3CR12; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED. ZINC PLATED STEEL. FABRICATION  METHOD: HOT","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,4000,4000,{"$nulls":3},8000,null,{"$f":"+T34*N34","v":0},0,{"$f":"T34*1.06","v":0},{"$f":"(W34*O34)","v":0},0,{"$f":"W34*1.06","v":0},{"$f":"(+Z34)*P34","v":0},0,0,{"$f":"(AC34)*Q34","v":0},0,{"$f":"AC34*1.06","v":0},{"$f":"(+AF34)*R34","v":0},0,{"$f":"AG34+AD34+AA34+X34+U34","v":0},0]
["Project Wagons 1000","914500236","PLATE METAL;6 MM,1565.6 MM,3400 MM",null,"PLATE, METALLIC; THICKNESS: 6 MM, WIDTH: 1565.6 MM, LENGTH: 3400 MM, MATERIAL GRADE: EN 10088 3CR12; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. ZINC PLATED STEEL. FABRICATION  METHOD: HOT ROLLED.  WIDTH UNTRIMMED","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,3062,3062,{"$nulls":3},6124,null,{"$f":"+T35*N35","v":0},0,{"$f":"T35*1.06","v":0},{"$f":"(W35*O35)","v":0},0,{"$f":"W35*1.06","v":0},{"$f":"(+Z35)*P35","v":0},0,0,{"$f":"(AC35)*Q35","v":0},0,{"$f":"AC35*1.06","v":0},{"$f":"(+AF35)*R35","v":0},0,{"$f":"AG35+AD35+AA35+X35+U35","v":0},0]
["Manufacturing","811380303","BAR METAL;DIA 10 X LG 6000 MM,RND",null,"BAR, METALLIC; DIMENSIONS: DIA 10 X LG 6000 MM, SHAPE: ROUND; MATERIAL GRADE NEW: AISI 304L; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED","BAR, ","M",null,"AISI SAE 304L","SST & 3CR12","Stainless Steel","Sections",null,135,135,135,135,135,675,null,{"$f":"+T36*N36","v":0},0,{"$f":"T36*1.06","v":0},{"$f":"(W36*O36)","v":0},0,{"$f":"W36*1.06","v":0},{"$f":"(+Z36)*P36","v":0},0,0,{"$f":"(AC36)*Q36","v":0},0,{"$f":"AC36*1.06","v":0},{"$f":"(+AF36)*R36","v":0},0,{"$f":"AG36+AD36+AA36+X36+U36","v":0},0]
["Manufacturing","914500220","PLATE METAL;4 MM,1500 MM,3410 MM",null,"PLATE, METALLIC; THICKNESS: 4 MM, WIDTH: 1500 MM, LENGTH: 3410 MM, MATERIAL GRADE: EN 10088 3CR12; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED. HRA","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,42,42,42,42,42,210,null,{"$f":"+T37*N37","v":0},0,{"$f":"T37*1.06","v":0},{"$f":"(W37*O37)","v":0},0,{"$f":"W37*1.06","v":0},{"$f":"(+Z37)*P37","v":0},0,0,{"$f":"(AC37)*Q37","v":0},0,{"$f":"AC37*1.06","v":0},{"$f":"(+AF37)*R37","v":0},0,{"$f":"AG37+AD37+AA37+X37+U37","v":0},0]
["Manufacturing","914500222","PLATE METAL;4 MM,1500 MM,2700 MM",null,"PLATE, METALLIC; THICKNESS: 4 MM, WIDTH: 1500 MM, LENGTH: 2700 MM, MATERIAL GRADE: EN 10088 3CR12; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED. IDENTIFICATION MUST BE STENCILLED","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,7,7,7,7,7,35,null,{"$f":"+T38*N38","v":0},0,{"$f":"T38*1.06","v":0},{"$f":"(W38*O38)","v":0},0,{"$f":"W38*1.06","v":0},{"$f":"(+Z38)*P38","v":0},0,0,{"$f":"(AC38)*Q38","v":0},0,{"$f":"AC38*1.06","v":0},{"$f":"(+AF38)*R38","v":0},0,{"$f":"AG38+AD38+AA38+X38+U38","v":0},0]
["Project Wagons 1000","914500220","PLATE METAL;4 MM,1500 MM,3410 MM",null,"PLATE, METALLIC; THICKNESS: 4 MM, WIDTH: 1500 MM, LENGTH: 3410 MM, MATERIAL GRADE: EN 10088 3CR12; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED. HRA","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,118,118,{"$nulls":3},236,null,{"$f":"+T39*N39","v":0},0,{"$f":"T39*1.06","v":0},{"$f":"(W39*O39)","v":0},0,{"$f":"W39*1.06","v":0},{"$f":"(+Z39)*P39","v":0},0,0,{"$f":"(AC39)*Q39","v":0},0,{"$f":"AC39*1.06","v":0},{"$f":"(+AF39)*R39","v":0},0,{"$f":"AG39+AD39+AA39+X39+U39","v":0},0]
["Project Wagons 1000","914500222","PLATE METAL;4 MM,1500 MM,2700 MM",null,"PLATE, METALLIC; THICKNESS: 4 MM, WIDTH: 1500 MM, LENGTH: 2700 MM, MATERIAL GRADE: EN 10088 3CR12; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED. IDENTIFICATION MUST BE STENCILLED","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,200,200,{"$nulls":3},400,null,{"$f":"+T40*N40","v":0},0,{"$f":"T40*1.06","v":0},{"$f":"(W40*O40)","v":0},0,{"$f":"W40*1.06","v":0},{"$f":"(+Z40)*P40","v":0},0,0,{"$f":"(AC40)*Q40","v":0},0,{"$f":"AC40*1.06","v":0},{"$f":"(+AF40)*R40","v":0},0,{"$f":"AG40+AD40+AA40+X40+U40","v":0},0]
["Manufacturing","811380291","BAR METAL;DIA 30 X LG 6000 MM,RND",null,"BAR, METALLIC; DIMENSIONS: DIA 30 X LG 6000 MM, SHAPE: ROUND; MATERIAL GRADE NEW: AISI 304; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED.","BAR, ","M",null,"AISI SAE 304L","SST & 3CR12","Stainless Steel","Sections",null,3199,3199,3199,3199,3199,15995,null,{"$f":"+T41*N41","v":0},0,{"$f":"T41*1.06","v":0},{"$f":"(W41*O41)","v":0},0,{"$f":"W41*1.06","v":0},{"$f":"(+Z41)*P41","v":0},0,0,{"$f":"(AC41)*Q41","v":0},0,{"$f":"AC41*1.06","v":0},{"$f":"(+AF41)*R41","v":0},0,{"$f":"AG41+AD41+AA41+X41+U41","v":0},0]
["Manufacturing","811300095","PLATE METAL;4.5 MM,1250 MM,2500 MM",null,"PLATE, METALLIC; THICKNESS: 4.5 MM, WIDTH: 1250 MM, LENGTH: 2500 MM, MATERIAL GRADE: EN10088 3CR12; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED. NO 1 FINISH.  MATERIAL DELIVERED KOEDOESPOO","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,34,34,34,34,34,170,null,{"$f":"+T42*N42","v":0},0,{"$f":"T42*1.06","v":0},{"$f":"(W42*O42)","v":0},0,{"$f":"W42*1.06","v":0},{"$f":"(+Z42)*P42","v":0},0,0,{"$f":"(AC42)*Q42","v":0},0,{"$f":"AC42*1.06","v":0},{"$f":"(+AF42)*R42","v":0},0,{"$f":"AG42+AD42+AA42+X42+U42","v":0},0]
["Manufacturing","011116702","PLATE METAL;6 MM,WD:2.125 M,LG:2.9 M,STL",null,"PLATE, METALLIC; THICKNESS: 6 MM, WIDTH: 2.125 M, LENGTH: 2.9 M, PLATE MATERIAL: STEEL, MATERIAL GRADE: 3CR12","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,5,5,11,16,16,53,null,{"$f":"+T43*N43","v":0},0,{"$f":"T43*1.06","v":0},{"$f":"(W43*O43)","v":0},0,{"$f":"W43*1.06","v":0},{"$f":"(+Z43)*P43","v":0},0,0,{"$f":"(AC43)*Q43","v":0},0,{"$f":"AC43*1.06","v":0},{"$f":"(+AF43)*R43","v":0},0,{"$f":"AG43+AD43+AA43+X43+U43","v":0},0]
["Manufacturing","011116703","PLATE METAL;6 MM,WD:2.125 M,LG:3.05 M",null,"PLATE, METALLIC; THICKNESS: 6 MM, WIDTH: 2.125 M, LENGTH: 3.05 M, PLATE MATERIAL: STEEL, MATERIAL GRADE: 3CR12","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,2,2,6,8,8,26,null,{"$f":"+T44*N44","v":0},0,{"$f":"T44*1.06","v":0},{"$f":"(W44*O44)","v":0},0,{"$f":"W44*1.06","v":0},{"$f":"(+Z44)*P44","v":0},0,0,{"$f":"(AC44)*Q44","v":0},0,{"$f":"AC44*1.06","v":0},{"$f":"(+AF44)*R44","v":0},0,{"$f":"AG44+AD44+AA44+X44+U44","v":0},0]
["Manufacturing","914400872","PLATE METAL;12 MM,1500 MM,4000 MM",null,"PLATE, METALLIC; THICKNESS: 12 MM, WIDTH: 1500 MM, LENGTH: 4000 MM, MATERIAL GRADE: EN 10088 3CR12; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED NO RUST OR CORROSION ON THE SURFACE ALLOWED","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,27,27,27,27,27,135,null,{"$f":"+T45*N45","v":0},0,{"$f":"T45*1.06","v":0},{"$f":"(W45*O45)","v":0},0,{"$f":"W45*1.06","v":0},{"$f":"(+Z45)*P45","v":0},0,0,{"$f":"(AC45)*Q45","v":0},0,{"$f":"AC45*1.06","v":0},{"$f":"(+AF45)*R45","v":0},0,{"$f":"AG45+AD45+AA45+X45+U45","v":0},0]
["Project Wagons 1000","914400872","PLATE METAL;12 MM,1500 MM,4000 MM",null,"PLATE, METALLIC; THICKNESS: 12 MM, WIDTH: 1500 MM, LENGTH: 4000 MM, MATERIAL GRADE: EN 10088 3CR12; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED NO RUST OR CORROSION ON THE SURFACE ALLOWED","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,70,70,{"$nulls":3},140,null,{"$f":"+T46*N46","v":0},0,{"$f":"T46*1.06","v":0},{"$f":"(W46*O46)","v":0},0,{"$f":"W46*1.06","v":0},{"$f":"(+Z46)*P46","v":0},0,0,{"$f":"(AC46)*Q46","v":0},0,{"$f":"AC46*1.06","v":0},{"$f":"(+AF46)*R46","v":0},0,{"$f":"AG46+AD46+AA46+X46+U46","v":0},0]
["Manufacturing","811380291","BAR METAL;DIA 30 X LG 6000 MM,RND",null,"BAR, METALLIC; DIMENSIONS: DIA 30 X LG 6000 MM, SHAPE: ROUND; MATERIAL GRADE NEW: AISI 304; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED.","BAR, ","M",null,"AISI SAE 304L","SST & 3CR12","Stainless Steel","Sections",null,934,927,260,260,260,2641,null,{"$f":"+T47*N47","v":0},0,{"$f":"T47*1.06","v":0},{"$f":"(W47*O47)","v":0},0,{"$f":"W47*1.06","v":0},{"$f":"(+Z47)*P47","v":0},0,0,{"$f":"(AC47)*Q47","v":0},0,{"$f":"AC47*1.06","v":0},{"$f":"(+AF47)*R47","v":0},0,{"$f":"AG47+AD47+AA47+X47+U47","v":0},0]
["Project Wagons 1000","811380291","BAR METAL;DIA 30 X LG 6000 MM,RND",null,"BAR, METALLIC; DIMENSIONS: DIA 30 X LG 6000 MM, SHAPE: ROUND; MATERIAL GRADE NEW: AISI 304; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED.","BAR, ","M",null,"AISI SAE 304L","SST & 3CR12","Stainless Steel","Sections",null,1220,1220,{"$nulls":3},2440,null,{"$f":"+T48*N48","v":0},0,{"$f":"T48*1.06","v":0},{"$f":"(W48*O48)","v":0},0,{"$f":"W48*1.06","v":0},{"$f":"(+Z48)*P48","v":0},0,0,{"$f":"(AC48)*Q48","v":0},0,{"$f":"AC48*1.06","v":0},{"$f":"(+AF48)*R48","v":0},0,{"$f":"AG48+AD48+AA48+X48+U48","v":0},0]
["Manufacturing","511420005","PLATE METAL;6 MM,1250 MM,2500 MM",null,"PLATE, METALLIC; THICKNESS: 6 MM, WIDTH: 1250 MM, LENGTH: 2500 MM, MATERIAL GRADE: EN10088 3CR12; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED. FABRICATION METHOD: HOT ROLLED ALLOY","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,251,167,293,385,267,1363,null,{"$f":"+T49*N49","v":0},0,{"$f":"T49*1.06","v":0},{"$f":"(W49*O49)","v":0},0,{"$f":"W49*1.06","v":0},{"$f":"(+Z49)*P49","v":0},0,0,{"$f":"(AC49)*Q49","v":0},0,{"$f":"AC49*1.06","v":0},{"$f":"(+AF49)*R49","v":0},0,{"$f":"AG49+AD49+AA49+X49+U49","v":0},0]
["Manufacturing","014002288","SHEET METAL;3CR12,STL,3 MM,1.25 M,2.5 M",null,"SHEET, METALLIC; MATERIAL GRADE: 3CR12, MATERIAL: STEEL, THICKNESS: 3 MM, WIDTH: 1.25 M, LENGTH: 2.5 M, SURFACE TREATMENT: NO 1 FIN E FINISH; CERTIFICATE TO BE SENT WITH MATERIAL; DELIVERED KOEDOESPOORT: MATERIAL MUST BE SUPPLIED FLAT STRAPPED TO A PALLET","SHEET","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,61,93,40,34,94,322,null,{"$f":"+T50*N50","v":0},0,{"$f":"T50*1.06","v":0},{"$f":"(W50*O50)","v":0},0,{"$f":"W50*1.06","v":0},{"$f":"(+Z50)*P50","v":0},0,0,{"$f":"(AC50)*Q50","v":0},0,{"$f":"AC50*1.06","v":0},{"$f":"(+AF50)*R50","v":0},0,{"$f":"AG50+AD50+AA50+X50+U50","v":0},0]
["Manufacturing","311200019","PLATE METAL;4.5 MM,1500 MM,2500 MM",null,"PLATE, METALLIC; THICKNESS: 4.5 MM, WIDTH: 1500 MM, LENGTH: 2500 MM; MATERIAL GRADE NEW:  EN 10088 3CR12 MATERIAL GRADE OLD: 3CR12; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED. HOT ROLLED","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,43,27,44,56,33,203,null,{"$f":"+T51*N51","v":0},0,{"$f":"T51*1.06","v":0},{"$f":"(W51*O51)","v":0},0,{"$f":"W51*1.06","v":0},{"$f":"(+Z51)*P51","v":0},0,0,{"$f":"(AC51)*Q51","v":0},0,{"$f":"AC51*1.06","v":0},{"$f":"(+AF51)*R51","v":0},0,{"$f":"AG51+AD51+AA51+X51+U51","v":0},0]
["Manufacturing","011006750","BAR METAL;WD 22 X LG 6000 X THK 3 MM",null,"BAR, METALLIC; DIMENSIONS: WD 22 X LG 6000 X THK 3 MM, SHAPE: FLAT; MATERIAL GRADE NEW: AISI 1045 MATERIAL GRADE OLD: BS 970 080A67 GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED. SPEC.CME 14","BAR, ","M",null,"AISI 1045","SST & 3CR12","Stainless Steel","Sections",null,494,316,503,633,385,2331,null,{"$f":"+T52*N52","v":0},0,{"$f":"T52*1.06","v":0},{"$f":"(W52*O52)","v":0},0,{"$f":"W52*1.06","v":0},{"$f":"(+Z52)*P52","v":0},0,0,{"$f":"(AC52)*Q52","v":0},0,{"$f":"AC52*1.06","v":0},{"$f":"(+AF52)*R52","v":0},0,{"$f":"AG52+AD52+AA52+X52+U52","v":0},0]
["Project Wagons 1000","011006750","BAR METAL;WD 22 X LG 6000 X THK 3 MM",null,"BAR, METALLIC; DIMENSIONS: WD 22 X LG 6000 X THK 3 MM, SHAPE: FLAT; MATERIAL GRADE NEW: AISI 1045 MATERIAL GRADE OLD: BS 970 080A67 GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED. SPEC.CME 14","BAR, ","M",null,"AISI 1045","SST & 3CR12","Stainless Steel","Sections",null,3200,3200,{"$nulls":3},6400,null,{"$f":"+T53*N53","v":0},0,{"$f":"T53*1.06","v":0},{"$f":"(W53*O53)","v":0},0,{"$f":"W53*1.06","v":0},{"$f":"(+Z53)*P53","v":0},0,0,{"$f":"(AC53)*Q53","v":0},0,{"$f":"AC53*1.06","v":0},{"$f":"(+AF53)*R53","v":0},0,{"$f":"AG53+AD53+AA53+X53+U53","v":0},0]
["Manufacturing","011670457","PLATE METAL;8 MM,1100 MM,3000 MM",null,"PLATE, METALLIC; THICKNESS: 8 MM, WIDTH: 1100 MM, LENGTH: 3000 MM, MATERIAL GRADE: EN 100088 3CR12; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED. HRA","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,47,47,104,149,152,499,null,{"$f":"+T54*N54","v":0},0,{"$f":"T54*1.06","v":0},{"$f":"(W54*O54)","v":0},0,{"$f":"W54*1.06","v":0},{"$f":"(+Z54)*P54","v":0},0,0,{"$f":"(AC54)*Q54","v":0},0,{"$f":"AC54*1.06","v":0},{"$f":"(+AF54)*R54","v":0},0,{"$f":"AG54+AD54+AA54+X54+U54","v":0},0]
["Manufacturing","611000267","PLATE METAL;12 MM,1290 MM,2580 MM",null,"PLATE, METALLIC; THICKNESS: 12 MM, WIDTH: 1290 MM, LENGTH: 2580 MM, MATERIAL GRADE: EN10088 3CR12; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED. FABRICATION METHOD: HOT ROLLED SPECIAL FEATU","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,95,95,95,95,95,475,null,{"$f":"+T55*N55","v":0},0,{"$f":"T55*1.06","v":0},{"$f":"(W55*O55)","v":0},0,{"$f":"W55*1.06","v":0},{"$f":"(+Z55)*P55","v":0},0,0,{"$f":"(AC55)*Q55","v":0},0,{"$f":"AC55*1.06","v":0},{"$f":"(+AF55)*R55","v":0},0,{"$f":"AG55+AD55+AA55+X55+U55","v":0},0]
["Manufacturing","011670459","PLATE METAL;5 MM,1524 MM,2200 MM",null,"PLATE, METALLIC; THICKNESS: 5 MM, WIDTH: 1524 MM, LENGTH: 2200 MM, MATERIAL GRADE: EN 100088 3CR12, SPECIAL FEATURES: PRECISION CUT; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED. PRECISION","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,9,9,21,30,30,99,null,{"$f":"+T56*N56","v":0},0,{"$f":"T56*1.06","v":0},{"$f":"(W56*O56)","v":0},0,{"$f":"W56*1.06","v":0},{"$f":"(+Z56)*P56","v":0},0,0,{"$f":"(AC56)*Q56","v":0},0,{"$f":"AC56*1.06","v":0},{"$f":"(+AF56)*R56","v":0},0,{"$f":"AG56+AD56+AA56+X56+U56","v":0},0]
["Manufacturing","514662979","SHEET METAL;EN10088 3CR12,STL,3 MM",null,"SHEET, METALLIC; MATERIAL GRADE: EN10088 3CR12, MATERIAL: STEEL, THICKNESS: 3 MM, WIDTH: 1250 MM, LENGTH: 2500 MM; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED. SURFACE CONDITION HRA","SHEET","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,11,11,25,35,36,118,null,{"$f":"+T57*N57","v":0},0,{"$f":"T57*1.06","v":0},{"$f":"(W57*O57)","v":0},0,{"$f":"W57*1.06","v":0},{"$f":"(+Z57)*P57","v":0},0,0,{"$f":"(AC57)*Q57","v":0},0,{"$f":"AC57*1.06","v":0},{"$f":"(+AF57)*R57","v":0},0,{"$f":"AG57+AD57+AA57+X57+U57","v":0},0]
["Manufacturing","011115803","PLATE METAL;10 MM,WD:1.5 M,LG:4.445 M",null,"PLATE, METALLIC; THICKNESS: 10 MM, WIDTH: 1.5 M, LENGTH: 4.445 M, PLATE MATERIAL: STEEL, MATERIAL GRADE: 3CR12 HRA","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,3,3,6,8,9,29,null,{"$f":"+T58*N58","v":0},0,{"$f":"T58*1.06","v":0},{"$f":"(W58*O58)","v":0},0,{"$f":"W58*1.06","v":0},{"$f":"(+Z58)*P58","v":0},0,0,{"$f":"(AC58)*Q58","v":0},0,{"$f":"AC58*1.06","v":0},{"$f":"(+AF58)*R58","v":0},0,{"$f":"AG58+AD58+AA58+X58+U58","v":0},0]
["Manufacturing","011670464","PLATE METAL;6 MM,1100 MM,3100 MM",null,"PLATE, METALLIC; THICKNESS: 6 MM, WIDTH: 1100 MM, LENGTH: 3100 MM, MATERIAL GRADE: EN 10088 3CR12; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,7,7,17,24,24,79,null,{"$f":"+T59*N59","v":0},0,{"$f":"T59*1.06","v":0},{"$f":"(W59*O59)","v":0},0,{"$f":"W59*1.06","v":0},{"$f":"(+Z59)*P59","v":0},0,0,{"$f":"(AC59)*Q59","v":0},0,{"$f":"AC59*1.06","v":0},{"$f":"(+AF59)*R59","v":0},0,{"$f":"AG59+AD59+AA59+X59+U59","v":0},0]
["Manufacturing","511420117","PLATE 3CR12  8x1300x2500 HRA",null,"PLATE 8x1300x2500 GRADE: 3CR12 (HRA) MUST BE DELIVERED WITH A MATERIAL CERTIFICATE","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,89,76,89,0,0,254,null,{"$f":"+T60*N60","v":0},0,{"$f":"T60*1.06","v":0},{"$f":"(W60*O60)","v":0},0,{"$f":"W60*1.06","v":0},{"$f":"(+Z60)*P60","v":0},0,0,{"$f":"(AC60)*Q60","v":0},0,{"$f":"AC60*1.06","v":0},{"$f":"(+AF60)*R60","v":0},0,{"$f":"AG60+AD60+AA60+X60+U60","v":0},0]
["Manufacturing","914500234","PLATE METAL;6 MM,1500 MM,3400 MM",null,"PLATE, METALLIC; THICKNESS: 6 MM, WIDTH: 1500 MM, LENGTH: 3400 MM, MATERIAL GRADE: EN 10088 3CR12; ZINC PLATED STEEL. FABRICATIONME THOD: HOT ROLLED. (PRECISION CUT) L = 3400 + 0-2 MM W = 1500 + 0-2 MM SQUARE = ± 0+2 MM.","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,0,190,190,190,190,760,null,{"$f":"+T61*N61","v":0},0,{"$f":"T61*1.06","v":0},{"$f":"(W61*O61)","v":0},0,{"$f":"W61*1.06","v":0},{"$f":"(+Z61)*P61","v":0},0,0,{"$f":"(AC61)*Q61","v":0},0,{"$f":"AC61*1.06","v":0},{"$f":"(+AF61)*R61","v":0},0,{"$f":"AG61+AD61+AA61+X61+U61","v":0},0]
["Project Wagons 1000","914500234","PLATE METAL;6 MM,1500 MM,3400 MM",null,"PLATE, METALLIC; THICKNESS: 6 MM, WIDTH: 1500 MM, LENGTH: 3400 MM, MATERIAL GRADE: EN 10088 3CR12; ZINC PLATED STEEL. FABRICATIONME THOD: HOT ROLLED. (PRECISION CUT) L = 3400 + 0-2 MM W = 1500 + 0-2 MM SQUARE = ± 0+2 MM.","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,532,532,{"$nulls":3},1064,null,{"$f":"+T62*N62","v":0},0,{"$f":"T62*1.06","v":0},{"$f":"(W62*O62)","v":0},0,{"$f":"W62*1.06","v":0},{"$f":"(+Z62)*P62","v":0},0,0,{"$f":"(AC62)*Q62","v":0},0,{"$f":"AC62*1.06","v":0},{"$f":"(+AF62)*R62","v":0},0,{"$f":"AG62+AD62+AA62+X62+U62","v":0},0]
["Manufacturing","011670462","PLATE METAL;5 MM,1524 MM,3048 MM",null,"PLATE, METALLIC; THICKNESS: 5 MM, WIDTH: 1524 MM, LENGTH: 3048 MM, MATERIAL GRADE: EN 100088 3CR12; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED. SPECIAL FEAUTURE: PRECISION CUT","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,118,118,264,376,384,1260,null,{"$f":"+T63*N63","v":0},0,{"$f":"T63*1.06","v":0},{"$f":"(W63*O63)","v":0},0,{"$f":"W63*1.06","v":0},{"$f":"(+Z63)*P63","v":0},0,0,{"$f":"(AC63)*Q63","v":0},0,{"$f":"AC63*1.06","v":0},{"$f":"(+AF63)*R63","v":0},0,{"$f":"AG63+AD63+AA63+X63+U63","v":0},0]
["Manufacturing","011673950","PLATE METAL;8 MM,788 MM,3020 MM,STL",null,"PLATE, METALLIC; THICKNESS: 8 MM, WIDTH: 788 MM, LENGTH: 3020 MM, PLATE MATERIAL: STEEL; MATERIAL GRADE NEW: EN 10088 3CR12; MATRIAL GRADE : 3CR12 HRA TOLERANCE +/- 1MM GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSIO","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,653,401,681,873,531,3139,null,{"$f":"+T64*N64","v":0},0,{"$f":"T64*1.06","v":0},{"$f":"(W64*O64)","v":0},0,{"$f":"W64*1.06","v":0},{"$f":"(+Z64)*P64","v":0},0,0,{"$f":"(AC64)*Q64","v":0},0,{"$f":"AC64*1.06","v":0},{"$f":"(+AF64)*R64","v":0},0,{"$f":"AG64+AD64+AA64+X64+U64","v":0},0]
["Manufacturing","011670461","PLATE METAL;5 MM,1524 MM,2800 MM",null,"PLATE, METALLIC; THICKNESS: 5 MM, WIDTH: 1524 MM, LENGTH: 2800 MM, MATERIAL GRADE: EN 100088 3CR12; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED. PRECISION CUT","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,209,209,466,664,679,2227,null,{"$f":"+T65*N65","v":0},0,{"$f":"T65*1.06","v":0},{"$f":"(W65*O65)","v":0},0,{"$f":"W65*1.06","v":0},{"$f":"(+Z65)*P65","v":0},0,0,{"$f":"(AC65)*Q65","v":0},0,{"$f":"AC65*1.06","v":0},{"$f":"(+AF65)*R65","v":0},0,{"$f":"AG65+AD65+AA65+X65+U65","v":0},0]
["Manufacturing","011673951","PLATE METAL;8 MM,788 MM,3098 MM",null,"PLATE, METALLIC; THICKNESS: 8 MM, WIDTH: 788 MM, LENGTH: 3098 MM, MATERIAL GRADE: EN 10088 3CR12; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED. HOT ROLLED ALLOYED (HRA)","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,526,321,536,684,401,2468,null,{"$f":"+T66*N66","v":0},0,{"$f":"T66*1.06","v":0},{"$f":"(W66*O66)","v":0},0,{"$f":"W66*1.06","v":0},{"$f":"(+Z66)*P66","v":0},0,0,{"$f":"(AC66)*Q66","v":0},0,{"$f":"AC66*1.06","v":0},{"$f":"(+AF66)*R66","v":0},0,{"$f":"AG66+AD66+AA66+X66+U66","v":0},0]
["Manufacturing","311111586","PLATE STEEL  8x1200x3200 HRA 3CR12",null,"PLATE STEEL (3CR12) 8x1200x3200 HRA SPEC. 3CR12 HRA MUST BE SUPPLIED WITH A MATERIAL CERTIFICATE","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,199,134,248,328,245,1154,null,{"$f":"+T67*N67","v":0},0,{"$f":"T67*1.06","v":0},{"$f":"(W67*O67)","v":0},0,{"$f":"W67*1.06","v":0},{"$f":"(+Z67)*P67","v":0},0,0,{"$f":"(AC67)*Q67","v":0},0,{"$f":"AC67*1.06","v":0},{"$f":"(+AF67)*R67","v":0},0,{"$f":"AG67+AD67+AA67+X67+U67","v":0},0]
["Manufacturing","311200021","PLATE METAL;10 MM,1500 MM,2500 MM",null,"PLATE, METALLIC; THICKNESS: 10 MM, WIDTH: 1500 MM, LENGTH: 2500 MM; MATERIAL GRADE NEW: EN 10088 3CR12 MATERIAL GRADE OLD: 3CR12 HRA; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED.","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,103,103,103,103,103,{"$f":"N68+O68+P68+Q68+R68","v":515},null,{"$f":"+T68*N68","v":0},{"$f":"U68*1.15","v":0},{"$f":"T68*1.06","v":0},{"$f":"(W68*O68)","v":0},{"$f":"X68*1.15","v":0},{"$f":"W68*1.06","v":0},{"$f":"(+Z68)*P68","v":0},{"$f":"AA68*1.15","v":0},{"$f":"Z68*1.06","v":0},{"$f":"(AC68)*Q68","v":0},{"$f":"AD68*1.15","v":0},{"$f":"AC68*1.06","v":0},{"$f":"(+AF68)*R68","v":0},{"$f":"AG68*1.15","v":0},{"$f":"AG68+AD68+AA68+X68+U68","v":0},{"$f":"AI68*1.15","v":0}]
["Manufacturing","611000249","PLATE METAL;4 MM,1040 MM,3000 MM,HOT RLD",null,"PLATE, METALLIC; THICKNESS: 4 MM, WIDTH: 1040 MM, LENGTH: 3000 MM, MATERIAL GRADE: EN 10088 3CR12, FABRICATION METHOD: HOT ROLLED; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,6,0,6,6,6,24,null,{"$f":"+T69*N69","v":0},0,{"$f":"T69*1.06","v":0},{"$f":"(W69*O69)","v":0},0,{"$f":"W69*1.06","v":0},{"$f":"(+Z69)*P69","v":0},0,0,{"$f":"(AC69)*Q69","v":0},0,{"$f":"AC69*1.06","v":0},{"$f":"(+AF69)*R69","v":0},0,{"$f":"AG69+AD69+AA69+X69+U69","v":0},0]
["Manufacturing","011009601","PLATE METAL;8 MM,2500 MM,1200 MM",null,"PLATE, METALLIC; THICKNESS: 8 MM, WIDTH: 2500 MM, LENGTH: 1200 MM; MATERIAL GRADE NEW: EN 10088 3CR12 MATERIAL GRADE OLD: EN 10088 3CR12; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED. MAX L","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,8,8,8,8,8,40,null,{"$f":"+T70*N70","v":0},0,{"$f":"T70*1.06","v":0},{"$f":"(W70*O70)","v":0},0,{"$f":"W70*1.06","v":0},{"$f":"(+Z70)*P70","v":0},0,0,{"$f":"(AC70)*Q70","v":0},0,{"$f":"AC70*1.06","v":0},{"$f":"(+AF70)*R70","v":0},0,{"$f":"AG70+AD70+AA70+X70+U70","v":0},0]
["Manufacturing","914500233","PLATE METAL;6 MM,1490 MM,2880 MM",null,"PLATE, METALLIC; THICKNESS: 6 MM, WIDTH: 1490 MM, LENGTH: 2880 MM, MATERIAL GRADE: EN 10088 3CR12; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. ZINC PLATED STEEL. FABRICATION METHOD: HOT ROLLED. (PRECISION CUT) L = 2880 + 0-2 MM W =","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,108,67,113,146,89,523,null,{"$f":"+T71*N71","v":0},0,{"$f":"T71*1.06","v":0},{"$f":"(W71*O71)","v":0},0,{"$f":"W71*1.06","v":0},{"$f":"(+Z71)*P71","v":0},0,0,{"$f":"(AC71)*Q71","v":0},0,{"$f":"AC71*1.06","v":0},{"$f":"(+AF71)*R71","v":0},0,{"$f":"AG71+AD71+AA71+X71+U71","v":0},0]
["Project Wagons 1000","914500233","PLATE METAL;6 MM,1490 MM,2880 MM",null,"PLATE, METALLIC; THICKNESS: 6 MM, WIDTH: 1490 MM, LENGTH: 2880 MM, MATERIAL GRADE: EN 10088 3CR12; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. ZINC PLATED STEEL. FABRICATION METHOD: HOT ROLLED. (PRECISION CUT) L = 2880 + 0-2 MM W =","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,1002,1002,{"$nulls":3},2004,null,{"$f":"+T72*N72","v":0},0,{"$f":"T72*1.06","v":0},{"$f":"(W72*O72)","v":0},0,{"$f":"W72*1.06","v":0},{"$f":"(+Z72)*P72","v":0},0,0,{"$f":"(AC72)*Q72","v":0},0,{"$f":"AC72*1.06","v":0},{"$f":"(+AF72)*R72","v":0},0,{"$f":"AG72+AD72+AA72+X72+U72","v":0},0]
["Manufacturing","511420115","PLATE METAL;4 MM,1500 MM,2500 MM",null,"PLATE, METALLIC; THICKNESS: 4 MM, WIDTH: 1500 MM, LENGTH: 2500 MM, MATERIAL GRADE: EN 10088 3CR12; GENERAL: MATERIAL CERTIFICATE TOEN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED. FABRICATION METHOD: HOT ROLLED. ZINC PLATED S","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,161,161,161,161,161,805,null,{"$f":"+T73*N73","v":0},0,{"$f":"T73*1.06","v":0},{"$f":"(W73*O73)","v":0},0,{"$f":"W73*1.06","v":0},{"$f":"(+Z73)*P73","v":0},0,0,{"$f":"(AC73)*Q73","v":0},0,{"$f":"AC73*1.06","v":0},{"$f":"(+AF73)*R73","v":0},0,{"$f":"AG73+AD73+AA73+X73+U73","v":0},0]
["Project Wagons 1000","511420115","PLATE METAL;4 MM,1500 MM,2500 MM",null,"PLATE, METALLIC; THICKNESS: 4 MM, WIDTH: 1500 MM, LENGTH: 2500 MM, MATERIAL GRADE: EN 10088 3CR12; GENERAL: MATERIAL CERTIFICATE TOEN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED. FABRICATION METHOD: HOT ROLLED. ZINC PLATED S","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,1945,1945,{"$nulls":3},3890,null,{"$f":"+T74*N74","v":0},0,{"$f":"T74*1.06","v":0},{"$f":"(W74*O74)","v":0},0,{"$f":"W74*1.06","v":0},{"$f":"(+Z74)*P74","v":0},0,0,{"$f":"(AC74)*Q74","v":0},0,{"$f":"AC74*1.06","v":0},{"$f":"(+AF74)*R74","v":0},0,{"$f":"AG74+AD74+AA74+X74+U74","v":0},0]
["Manufacturing","311201501","PLATE METAL;6 MM,1200 MM,2500 MM",null,"PLATE, METALLIC; THICKNESS: 6 MM, WIDTH: 1200 MM, LENGTH: 2500 MM, MATERIAL GRADE: EN10088 3CR12; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED.","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,93,98,191,268,283,933,null,{"$f":"+T75*N75","v":0},0,{"$f":"T75*1.06","v":0},{"$f":"(W75*O75)","v":0},0,{"$f":"W75*1.06","v":0},{"$f":"(+Z75)*P75","v":0},0,0,{"$f":"(AC75)*Q75","v":0},0,{"$f":"AC75*1.06","v":0},{"$f":"(+AF75)*R75","v":0},0,{"$f":"AG75+AD75+AA75+X75+U75","v":0},0]
["Manufacturing","013011120","PIPE METAL;PIPE SZ:ID 20 MM,6000 MM",null,"PIPE, METALLIC; PIPE SIZE: ID 20 MM, LENGTH: 6000 MM, WALL THICKNESS: 2.8 MM, PIPE MATERIAL: HEAVY BLACK; MATERIAL GRADE NEW: ASTM A106 GRB MATERIAL GRADE OLD:  BS1387 ASTM A106; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST O","PIPE,","M",null,"ASTM A106","SST & 3CR12","Stainless Steel","Pipe & Tube",null,111,96,157,200,186,750,null,{"$f":"+T76*N76","v":0},0,{"$f":"T76*1.06","v":0},{"$f":"(W76*O76)","v":0},0,{"$f":"W76*1.06","v":0},{"$f":"(+Z76)*P76","v":0},0,0,{"$f":"(AC76)*Q76","v":0},0,{"$f":"AC76*1.06","v":0},{"$f":"(+AF76)*R76","v":0},0,{"$f":"AG76+AD76+AA76+X76+U76","v":0},0]
["Manufacturing","914500578","PLATE METAL;4 MM,1500 MM,3300 MM",null,"PLATE, METALLIC; THICKNESS: 4 MM, WIDTH: 1500 MM, LENGTH: 3300 MM, MATERIAL GRADE: EN 10088 3CR12; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED. FABRICATION METHOD: HOT ROLLED","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,504,504,504,504,504,2520,null,{"$f":"+T77*N77","v":0},0,{"$f":"T77*1.06","v":0},{"$f":"(W77*O77)","v":0},0,{"$f":"W77*1.06","v":0},{"$f":"(+Z77)*P77","v":0},0,0,{"$f":"(AC77)*Q77","v":0},0,{"$f":"AC77*1.06","v":0},{"$f":"(+AF77)*R77","v":0},0,{"$f":"AG77+AD77+AA77+X77+U77","v":0},0]
["Manufacturing","611000253","PLATE METAL;4.5 MM,1290 MM,2500 MM",null,"PLATE, METALLIC; THICKNESS: 4.5 MM, WIDTH: 1290 MM, LENGTH: 2500 MM, MATERIAL GRADE: EN10088 3CR12; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED. FABRICATION METHOD: HOT ROLLED","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,38,38,38,38,38,190,null,{"$f":"+T78*N78","v":0},0,{"$f":"T78*1.06","v":0},{"$f":"(W78*O78)","v":0},0,{"$f":"W78*1.06","v":0},{"$f":"(+Z78)*P78","v":0},0,0,{"$f":"(AC78)*Q78","v":0},0,{"$f":"AC78*1.06","v":0},{"$f":"(+AF78)*R78","v":0},0,{"$f":"AG78+AD78+AA78+X78+U78","v":0},0]
["Manufacturing","611000254","PLATE METAL;6 MM,1290 MM,2500 MM",null,"PLATE, METALLIC; THICKNESS: 6 MM, WIDTH: 1290 MM, LENGTH: 2500 MM, MATERIAL GRADE: EN10088 3CR12; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED. FABRICATION METHOD: HOT ROLLED, SPECIAL FEATU","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,20,20,20,20,20,100,null,{"$f":"+T79*N79","v":0},0,{"$f":"T79*1.06","v":0},{"$f":"(W79*O79)","v":0},0,{"$f":"W79*1.06","v":0},{"$f":"(+Z79)*P79","v":0},0,0,{"$f":"(AC79)*Q79","v":0},0,{"$f":"AC79*1.06","v":0},{"$f":"(+AF79)*R79","v":0},0,{"$f":"AG79+AD79+AA79+X79+U79","v":0},0]
["Project Wagons 1000","611000253","PLATE METAL;4.5 MM,1290 MM,2500 MM",null,"PLATE, METALLIC; THICKNESS: 4.5 MM, WIDTH: 1290 MM, LENGTH: 2500 MM, MATERIAL GRADE: EN10088 3CR12; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED. FABRICATION METHOD: HOT ROLLED","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,14,14,{"$nulls":3},28,null,{"$f":"+T80*N80","v":0},0,{"$f":"T80*1.06","v":0},{"$f":"(W80*O80)","v":0},0,{"$f":"W80*1.06","v":0},{"$f":"(+Z80)*P80","v":0},0,0,{"$f":"(AC80)*Q80","v":0},0,{"$f":"AC80*1.06","v":0},{"$f":"(+AF80)*R80","v":0},0,{"$f":"AG80+AD80+AA80+X80+U80","v":0},0]
["Manufacturing","611000251","PLATE METAL;8 MM,1290 MM,2600 MM",null,"PLATE, METALLIC; THICKNESS: 8 MM, WIDTH: 1290 MM, LENGTH: 2600 MM, MATERIAL GRADE: EN10088 3CR12; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED FABRICATION METHOD: HOT  ROLLED","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,20,20,20,20,20,100,null,{"$f":"+T81*N81","v":0},0,{"$f":"T81*1.06","v":0},{"$f":"(W81*O81)","v":0},0,{"$f":"W81*1.06","v":0},{"$f":"(+Z81)*P81","v":0},0,0,{"$f":"(AC81)*Q81","v":0},0,{"$f":"AC81*1.06","v":0},{"$f":"(+AF81)*R81","v":0},0,{"$f":"AG81+AD81+AA81+X81+U81","v":0},0]
["Manufacturing","811300099","SHEET METAL;THK 4.5,WD 1.5M, LG 6M 3CR12",null,"SHEET, METALLIC TYPE PLATE THICKNESS 4.5 WIDTH 1.5 M LENGTH 6 M MATERIAL STEEL MATERIAL GRADE 3CR12 NO 1 FINISH CERTIFICATE TO BE SENT WITH MATERIAL DELIVERED KOEDOESPOORT: MATERIAL MUST BE SUPPLIED FLAT STRAPPED TO A PALLET THE MATERIAL MUST BE RUST FREE","SHEET","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,132,113,132,0,0,377,null,{"$f":"+T82*N82","v":0},0,{"$f":"T82*1.06","v":0},{"$f":"(W82*O82)","v":0},0,{"$f":"W82*1.06","v":0},{"$f":"(+Z82)*P82","v":0},0,0,{"$f":"(AC82)*Q82","v":0},0,{"$f":"AC82*1.06","v":0},{"$f":"(+AF82)*R82","v":0},0,{"$f":"AG82+AD82+AA82+X82+U82","v":0},0]
["Manufacturing","611000250","PLATE METAL;6 MM,1565 MM,1700 MM",null,"PLATE, METALLIC; THICKNESS: 6 MM, WIDTH: 1565 MM, LENGTH: 1700 MM, MATERIAL GRADE: EN 10088 3CR12; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,3,3,3,3,3,15,null,{"$f":"+T83*N83","v":0},0,{"$f":"T83*1.06","v":0},{"$f":"(W83*O83)","v":0},0,{"$f":"W83*1.06","v":0},{"$f":"(+Z83)*P83","v":0},0,0,{"$f":"(AC83)*Q83","v":0},0,{"$f":"AC83*1.06","v":0},{"$f":"(+AF83)*R83","v":0},0,{"$f":"AG83+AD83+AA83+X83+U83","v":0},0]
["Manufacturing","611000252","PLATE METAL;10 MM,2500 MM,1290 MM",null,"PLATE, METALLIC; THICKNESS: 10 MM, WIDTH: 2500 MM, LENGTH: 1290 MM, MATERIAL GRADE: EN10088 3CR12; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED. FABRICATION METHOD: HOT ROLLED, SPECIAL FEAT","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,4,4,4,4,4,20,null,{"$f":"+T84*N84","v":0},0,{"$f":"T84*1.06","v":0},{"$f":"(W84*O84)","v":0},0,{"$f":"W84*1.06","v":0},{"$f":"(+Z84)*P84","v":0},0,0,{"$f":"(AC84)*Q84","v":0},0,{"$f":"AC84*1.06","v":0},{"$f":"(+AF84)*R84","v":0},0,{"$f":"AG84+AD84+AA84+X84+U84","v":0},0]
["Manufacturing","011675468","PLATE METAL;5 MM,1.195 M,4.665 M,STL",null,"PLATE, METALLIC; THICKNESS: 5 MM, WIDTH: 1.195 M, LENGTH: 4.665 M, PLATE MATERIAL: STEEL, MATERIAL GRADE: 3CR12 BLACK UNPOLISHED, S PECIAL FEATURES: PRECISION CUT +/- 1 MM TOLERANCE","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,201,124,205,262,153,945,null,{"$f":"+T85*N85","v":0},0,{"$f":"T85*1.06","v":0},{"$f":"(W85*O85)","v":0},0,{"$f":"W85*1.06","v":0},{"$f":"(+Z85)*P85","v":0},0,0,{"$f":"(AC85)*Q85","v":0},0,{"$f":"AC85*1.06","v":0},{"$f":"(+AF85)*R85","v":0},0,{"$f":"AG85+AD85+AA85+X85+U85","v":0},0]
["Manufacturing","011675467","PLATE METAL;5 MM,773 MM,4.665 M,STL",null,"PLATE, METALLIC; THICKNESS: 5 MM, WIDTH: 773 MM, LENGTH: 4.665 M, PLATE MATERIAL: STEEL, MATERIAL GRADE: 3CR12, SPECIAL FEATURES: P RECISION CUT +/- 1 MM TOLERANCE","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,201,124,205,263,153,946,null,{"$f":"+T86*N86","v":0},0,{"$f":"T86*1.06","v":0},{"$f":"(W86*O86)","v":0},0,{"$f":"W86*1.06","v":0},{"$f":"(+Z86)*P86","v":0},0,0,{"$f":"(AC86)*Q86","v":0},0,{"$f":"AC86*1.06","v":0},{"$f":"(+AF86)*R86","v":0},0,{"$f":"AG86+AD86+AA86+X86+U86","v":0},0]
["Manufacturing","611000165","PLATE METAL;6 MM,1565 MM,3500 MM",null,"PLATE, METALLIC; THICKNESS: 6 MM, WIDTH: 1565 MM, LENGTH: 3500 MM, MATERIAL GRADE: EN10088 3CR12; N/B TOLERANCE  +/- 2MM GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED. FABRICATION METHOD: HO","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,260,160,265,339,198,1222,null,{"$f":"+T87*N87","v":0},0,{"$f":"T87*1.06","v":0},{"$f":"(W87*O87)","v":0},0,{"$f":"W87*1.06","v":0},{"$f":"(+Z87)*P87","v":0},0,0,{"$f":"(AC87)*Q87","v":0},0,{"$f":"AC87*1.06","v":0},{"$f":"(+AF87)*R87","v":0},0,{"$f":"AG87+AD87+AA87+X87+U87","v":0},0]
["Manufacturing","014001930","BAR METAL;DIA 20 X LG 6000 MM,RND",null,"BAR, METALLIC; DIMENSIONS: DIA 20 X LG 6000 MM, SHAPE: ROUND; MATERIAL GRADE NEW: AISI SAE 316L\nMATERIAL GRADE OLD: GRADE 316;\nGENE RAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED.  FABRICATION ME","BAR, ","M",null,"AISI SAE 316L","SST & 3CR12","Stainless Steel","Sections",null,255,254,186,99,86,880,null,{"$f":"+T88*N88","v":0},0,{"$f":"T88*1.06","v":0},{"$f":"(W88*O88)","v":0},0,{"$f":"W88*1.06","v":0},{"$f":"(+Z88)*P88","v":0},0,0,{"$f":"(AC88)*Q88","v":0},0,{"$f":"AC88*1.06","v":0},{"$f":"(+AF88)*R88","v":0},0,{"$f":"AG88+AD88+AA88+X88+U88","v":0},0]
["Manufacturing","013001224","PIPE METAL;SMLS,PIPE SZ:ID 32 MM,6000 MM",null,"PIPE, METALLIC; TYPE: SEAMLESS, PIPE SIZE: ID 32 MM, LENGTH: 6000 MM, WALL THICKNESS: 3.5 MM, PIPE MATERIAL: STEEL, SCHEDULE: 40, S PECIAL FEATURES: INTERNAL WELD BEAD REMOVED; MATERIAL GRADE NEW: ASTM A106 GRB\nMATERIAL GRADE OLD: BS1387 ASTM A106;\nGENERA","PIPE,","M",null,"ASTM A106","SST & 3CR12","Stainless Steel","Pipe & Tube",null,365,325,517,635,644,2486,null,{"$f":"+T89*N89","v":0},0,{"$f":"T89*1.06","v":0},{"$f":"(W89*O89)","v":0},0,{"$f":"W89*1.06","v":0},{"$f":"(+Z89)*P89","v":0},0,0,{"$f":"(AC89)*Q89","v":0},0,{"$f":"AC89*1.06","v":0},{"$f":"(+AF89)*R89","v":0},0,{"$f":"AG89+AD89+AA89+X89+U89","v":0},0]
["Manufacturing","114000291","SHEET METAL;STL,3 MM,1500 MM,3000 MM",null,"SHEET, METALLIC; MATERIAL GRADE: NEW: EN 10088 3CR12, OLD GRADE 3CR12, MATERIAL: STEEL, THICKNESS: 3 MM, WIDTH: 1500 MM, LENGTH: 30 00 MM; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWE","SHEET","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,448,459,44,56,44,1051,null,{"$f":"+T90*N90","v":0},{"$f":"U90*1.15","v":0},{"$f":"T90*1.06","v":0},{"$f":"(W90*O90)","v":0},{"$f":"X90*1.15","v":0},{"$f":"W90*1.06","v":0},{"$f":"(+Z90)*P90","v":0},{"$f":"AA90*1.15","v":0},{"$f":"Z90*1.06","v":0},{"$f":"(AC90)*Q90","v":0},{"$f":"AD90*1.15","v":0},{"$f":"AC90*1.06","v":0},{"$f":"(+AF90)*R90","v":0},{"$f":"AG90*1.15","v":0},{"$f":"AG90+AD90+AA90+X90+U90","v":0},{"$f":"AI90*1.15","v":0}]
["Project Wagons 1000","114000291","SHEET METAL;STL,3 MM,1500 MM,3000 MM",null,"SHEET, METALLIC; MATERIAL GRADE: NEW: EN 10088 3CR12, OLD GRADE 3CR12, MATERIAL: STEEL, THICKNESS: 3 MM, WIDTH: 1500 MM, LENGTH: 30 00 MM; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWE","SHEET","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,1000,1000,{"$nulls":3},2000,null,{"$f":"+T91*N91","v":0},0,{"$f":"T91*1.06","v":0},{"$f":"(W91*O91)","v":0},0,{"$f":"W91*1.06","v":0},{"$f":"(+Z91)*P91","v":0},0,0,{"$f":"(AC91)*Q91","v":0},0,{"$f":"AC91*1.06","v":0},{"$f":"(+AF91)*R91","v":0},0,{"$f":"AG91+AD91+AA91+X91+U91","v":0},0]
["Project Wagons 1000","311200021","PLATE METAL;10 MM,1500 MM,2500 MM",null,"PLATE, METALLIC; THICKNESS: 10 MM, WIDTH: 1500 MM, LENGTH: 2500 MM; MATERIAL GRADE NEW: EN 10088 3CR12 MATERIAL GRADE OLD: 3CR12 HRA; GENERAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED.","PLATE","EA",null,"EN 10088 3CR12","SST & 3CR12","Utility ferritic Stainless Steel ","Plates & Sheets",null,532,532,{"$nulls":3},1064,null,{"$f":"+T92*N92","v":0},0,{"$f":"T92*1.06","v":0},{"$f":"(W92*O92)","v":0},0,{"$f":"W92*1.06","v":0},{"$f":"(+Z92)*P92","v":0},0,0,{"$f":"(AC92)*Q92","v":0},0,{"$f":"AC92*1.06","v":0},{"$f":"(+AF92)*R92","v":0},0,{"$f":"AG92+AD92+AA92+X92+U92","v":0},0]
["Project Wagons 1000","014001930","BAR METAL;DIA 20 X LG 6000 MM,RND",null,"BAR, METALLIC; DIMENSIONS: DIA 20 X LG 6000 MM, SHAPE: ROUND; MATERIAL GRADE NEW: AISI SAE 316L\nMATERIAL GRADE OLD: GRADE 316;\nGENE RAL: MATERIAL CERTIFICATE TO EN 10204 TYPE 3.1 TO BE SUPPLIED. NO RUST OR CORROSION ON THE SURFACE ALLOWED.  FABRICATION ME","BAR, ","M",null,"AISI SAE 316L","SST & 3CR12","Stainless Steel","Sections",null,1200,1200,{"$nulls":3},2400,null,{"$f":"+T93*N93","v":0},0,{"$f":"T93*1.06","v":0},{"$f":"(W93*O93)","v":0},0,{"$f":"W93*1.06","v":0},{"$f":"(+Z93)*P93","v":0},0,0,{"$f":"(AC93)*Q93","v":0},0,{"$f":"AC93*1.06","v":0},{"$f":"(+AF93)*R93","v":0},0,{"$f":"AG93+AD93+AA93+X93+U93","v":0},0]
["I hereby acknowledge as a bidder that I have read and understood all the contents of this Purchase Order Long text Description . Furthermore, I (bidder) certifies and guarantees acceptance and compliance with this specification. Total value of these items must be carried over to page 33 of the RFP document.\n                                                                                                                                                                                                                                                                                                                                                                                         SIGNED THIS DAY _______________________ AT_________________________________\n                                                                                                                                                                                                                                                                                                        BY________________________________________________ (Full name in block letters)\n                                                                                                                                                                                                                                                                                                                                                                                                    IN MY CAPACITY AS ___________________________________ (Official designation)\n                                                                                                                                                                                                                                                                                                                                                                                               FOR THE COMPANY ___________________________________\n\nSIGNED _____________________________________________\n                                                                                                                                                                                                                                                                                                                                                                                            PLEASE NOTE: A Bidder must sign on the above and return this page together with a quote. "]