{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":8,"n_cols":2,"rows_kept":8}
["Material number","Purchase Order Long Text"]
["009839303","CLEANING COMPOUND, SOLVENT; TYPE: BASE DEGREASER, PACKAGE TYPE: DRUM 20 L; PROFLEX/DEGREASER 2 AND 3 BIODEGRADABLE SOLVENT BASE, NON-TOXIC TO HUMAN LIFE AND TO THE ENVIRONMENT, NON-FLAMMABLE; MUST NOT HLOROETHYLENE AND CRESYLIC ACID; FUNCTION: MUST REMOVE HIGH VISCOCITY OILS, CARBON DEPOSITS, DIRT, A (CRATER), SOILS FROM COMPONENTS WITHOUT DAMAGING THE COMPONENT'S SURFACE; OURDOR: VERY SLIGHT OUDOR, EYES, NOSE AND SENSES, NO FUMES; THE DEGREASER MUST BE ACCOMPANIED BY AN MSDS AND SILUTION RATIOS; HE SAME AS THE ONE THAT WAS SUPPLIED FOR SAMPLE TESTING AS PER REPORT: PD_COMP_NAT_RE_(INTERNAL USE) H TO THE METAL SURFACE AND MUST NOT CAUSE ANY CORROSIN, IT WILL BE ADVANTAGEOUS IF THE CHEMICAL CONT LIER MUST STATE SO;  MUST BE DISCHARGEABLE TO THE SEWAGE LINE AND CONFORM TO MUNICIPALITY DISCHARGE UENT; THE SUPPLIER MUST SUBMIT MATERIAL DATA SHEET, TECHNICAL DATA SHEET, BATCH CERTIFICATE AND A CE Y BATCH DELIVERED. NO BATCH WILL BE ACCPETED WITH THESE DOCUMENTS"]
["809200519","SOLVENT;TYPE: ELECTRICAL CLEANER,CONTAINER TYPE: DRUM,CONTAINER CAPACITY: 20 L,PHYSICAL FORM: LIQUID;SPECIFICATION: PD_COMP_NAT_SPEC_1026, LA;FUNCTION: IT MUST EFFECTIVELY REMOVE ALL CONTAMINANTS SUCH AS DIRT, OIL,OXIDES, FLUX, AND CARBON DEPOSITS FROM THE ELECTRICAL COMPONENTS TO AVOID SHORT CIRCUIT AND CORROSION;PROPERTIES: MUST ALIGN TO TRANSNET TECHNICAL SPECIFICATION: PD_COMP_N AT_SPEC_1026. IT MUST BE SAFE TO USE ON ALL METALS. MUST HAVE NO DETRIMENTAL EFFECT TO THE INSULATION MATERIAL. MUST BE: FAST DRYING, NON-FLAMMABLE,NON-CONDUCTIVE,  NON-CORROSIVE,A NON-OZONE DEPLETING SUBSTANCE (I.E IT MUST BE A FREE OF CHLORINATED SOLVENTS, CFCS, HCFC-225, HCFC 141B, HFES, PFCS, PERCHLOROETHYLENE AND NPB), NON-HARMFUL TO HUMANS WITH THE CORRECT PROTECTIVE CLOTHING USED;APPLICATION: CAN BE AEROSOL OR AS A SOLUTION THAT CAN BE USED TO SPRAY OR DIP COMPONENTS; OUDOR: VERY SLIGHT OUDOR, MUST NOT BE IRRITABLE TO HUMAN NOISE AND SENSES. NO FLUMES; CAPACITY: 20 L DEPENDING ON LIQUID STATE AND PACKAGING; REQUIRED DOCUMENTATION: BIDDER MUST SUBMIT TECHNICAL DATA SHEETS (TDS), MATERIAL SAFETY DATA SHEET (MSDS), AND CERTIFICATE OF ANALYSIS (COA). PLEASE NOTE ON DELIVERY A BATCH CERTIFICATE WITH THE COA MUST BE DELIVERED"]
[]
["Company Name"]
["Representative"]
["Date"]
["Signature"]