{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["A&B Schedules","Deviation Schedule","Test Schedule"],"not_rendered":{"defined_names":2},"read":"whole","date_system":"1900"}

{"sheet":"A&B Schedules","index":0,"n_rows":55,"n_cols":7,"rows_kept":55,"merged":[[0,1,0,6],[1,1,1,6],[2,1,2,6],[3,1,3,6],[4,1,4,6],[7,2,7,3],[8,2,8,3],[9,3,9,4],[19,3,19,4],[27,2,27,4],[28,2,28,5],[29,3,29,4],[34,3,34,4],[39,3,39,4],[43,3,43,4],[47,1,47,6],[50,1,50,3],[50,5,50,6],[54,1,54,3],[54,5,54,6]]}
[null,"Technical Schedules A and B for"]
[null,"STAYROD 1500xM12 34kN NON-ADJUST ESKOM DDT3011"]
[null,"ESKOM SAP No. 0163396"]
[null,"Schedule A:  Purchasers specific requirements"]
[null,"Schedule B:  Guarantees and technical particulars of equipment offered"]
[]
[null,1,null,2,null,3,4]
[null,"Item ","Description",null,null,"Schedule A","Schedule B"]
[null,1,"Product Information"]
[null,1.1,"·","Purchasing details"]
[null,"1.1.1",null,"Eskom SAP No",null,{"v":163396,"d":"0163396"},"xxxxxxxxxx"]
[null,"1.1.2",null,"Manufacturer's Name","Manufacturer Name","xxxxxxxxxx"]
[null,"1.1.3",null,"Manufacturer's Product Code","Specify Code","xxxxxxxxxx"]
[null,"1.1.4",null,"Manufacturer's Drawing number & Revision number","Specify No and Rev","xxxxxxxxxx"]
[null,"1.1.5",null,"Manufacturer's Physical identification mark indelible on product body","Specify Markings","xxxxxxxxxx"]
[null,"1.1.6",null,"Compliance to all dimensions and requirements of Eskom Buyer's Guide Drawings","Eskom DDT3011 and Eskom DDT3172","YES"]
[null,"1.1.7",null,"Item sample required, upon request from Eskom. (As per the Technical Criteria Document)",null,"YES","xxxxxxxxxx"]
[null,"1.1.8",null,"Stayrod to be compatible with: \nM12 Stay Plate - 0163417 (SEE Eskom DDT 3172 FOR DETAILS) (stay plate not included in supply of stay rod)","Eskom DDT 3172","YES","xxxxxxxxxx"]
[]
[null,1.2,"·","Mechanical Properties"]
[null,"1.2.1",null,"Mechanical failing load","kN",34]
[null,"1.2.2",null,"Material Grade as per EN10025-2 (European Standard)",null,"S275JR Steel"]
[null,"1.2.3",null,"Testing will be done to confirm the impact resistance at time of production for new production runs - minimum impact energy value of 27 J at 0 degree Celsius (Charpy V-Notch)\n",null,"YES"]
[]
[null,1.3,"·","Galvanising (where applicalbe)"]
[null,"1.3.1",null,"Average minimum galvanising thickness on product body complies to SANS 121","Hot Dipped","YES"]
[]
[null,2,"Documentation (to be submitted with tender)"]
[]
[null,2.1,"·","General"]
[null,"2.1.1",null,"Manufacturer's outline drawings of item","Sets",1]
[null,"2.1.2",null,"Material grade certification",null,"YES"]
[null,"2.1.3",null,"Visual inspection of welds","As per Eskom 240-75883830","YES"]
[]
[null,2.2,"·","Test Reports (where applicable)",null,"Required","Type Test in Submission"]
[null,"2.2.1",null,"Dimensional and material verification (SANS 61284)","Test report submitted","YES"]
[null,"2.2.2",null,"Galvanising certificate of product body (SANS 61284 and SANS 121)","Test report submitted","YES"]
[null,"2.2.3",null,"Visual examination  (SANS 61284)","Test report submitted","YES"]
[]
[null,2.3,"·","Mechanical Tests ",null,"Required","Type Test in Submission"]
[null,"2.3.1",null,"Tensile test (SANS 61284 and Eskom 10TB – 034) (Showing results for SMDL = 60% of SMFL and 100% SMFL as per 10TB – 034)","Test report submitted","YES"]
[null,"2.3.2",null,"Impact test (240-75883830) - Charpy V-Notch for off the shelf products (3.2.2.2 - minimum impact energy value of 27 J at 0 degree Celsius)","Test report submitted","YES or N/A for offers that will require a new production run"]
[]
[null,3,"·","Packaging"]
[null,3.1,null,"Packaging material, method and maximum quantity, not exceeding 50 units or 800kg (as per clause 4.18 of Eskom 240-60777474)","Wooden Boxes, Crates or Pallets, Hessian / Cloth Bags ","YES"]
[]
[]
[null,"SUPPLIER SIGNATURES"]
[]
[null,"         "]
[null,"Name (Print)",{"$nulls":3},"Company Name"]
[]
[]
[]
[null,"Sign",{"$nulls":3},"Date"]

{"sheet":"Deviation Schedule","index":1,"n_rows":43,"n_cols":6,"rows_kept":43,"merged":[[0,0,0,6],[1,0,1,6],[2,0,2,6],[3,0,3,6],[4,2,4,6],[5,2,5,6],[6,2,6,6],[7,2,7,6],[8,2,8,6],[9,2,9,6],[10,2,10,6],[11,2,11,6],[12,2,12,6],[13,2,13,6],[14,2,14,6],[15,2,15,6],[16,2,16,6],[17,2,17,6],[18,2,18,6],[19,2,19,6],[20,2,20,6],[21,2,21,6],[22,2,22,6],[23,2,23,6],[24,2,24,6],[25,2,25,6],[26,2,26,6],[27,2,27,6],[28,2,28,6],[29,2,29,6],[30,2,30,6],[31,2,31,6],[32,2,32,6],[33,2,33,6],[35,1,35,6],[38,1,38,3],[38,5,38,6],[42,1,42,3],[42,5,42,6],[45,0,45,1],[46,0,46,1]]}
["Deviation schedule"]
["STAYROD 1500xM12 34kN NON-ADJUST ESKOM DDT3011"]
["ESKOM SAP No. 0163396"]
["Deviations offered to this specification shall be listed below with reasons for deviation. This includes deviations on the AB Schedules, Drawings and Test Reports. In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective that that specified by Eskom."]
["Item","Clause","Description of Deviation"]
{"$rows_empty":30}
[null,"SUPPLIER SIGNATURES"]
[]
[null,"         "]
[null,"Name (Print)",{"$nulls":3},"Company Name"]
[]
[]
[]
[null,"Sign",{"$nulls":3},"Date"]

{"sheet":"Test Schedule","index":2,"n_rows":27,"n_cols":5,"rows_kept":27,"merged":[[0,1,0,4],[1,1,1,4],[2,1,2,4],[4,1,6,4],[8,1,8,4],[19,0,19,5],[22,0,22,2],[22,4,22,5],[26,0,26,2],[26,4,26,5]]}
[null,"Test Report Schedule"]
[null,"STAYROD 1500xM12 34kN NON-ADJUST ESKOM DDT3011"]
[null,"ESKOM SAP No. 0163396"]
[]
[null,"Important!\nCheck your submission to ensure that the specific test result for the specific tests stipulated can be found in the submission. Missing tests will affect the technical result."]
[]
[]
[]
[]
[null,1,2,3,4]
[null,"Item ","Description","Specification","Report No."]
[null,"2.2.1","Dimensional and material verification","SANS 61284"]
[null,"2.2.2","Galvanising certificate of product body","SANS 61284 and SANS 121"]
[null,"2.2.3","Visual examination ","SANS 61284"]
[null,"2.3.1","Tensile test (SANS 61284 and Eskom 10TB – 034) (Showing results for SMDL = 60% of SMFL and100% SMFL as per 10TB – 034)","SANS 61284 and Eskom 10TB – 034"]
[null,"2.3.2","Impact test (240-75883830) - Charpy V-Notch for off the shelf products (3.2.2.2 - minimum impact energy value of 27 J at 0 degree Celsius)","240-75883830"]
[]
[]
[]
["SUPPLIER SIGNATURES"]
[]
["         "]
["Name (Print)",{"$nulls":3},"Company Name"]
[]
[]
[]
["Sign",{"$nulls":3},"Date"]