Specs for RFQ: ITS012509RFQ00000051

1. ELECTRODE PH FLOW GLASS REFILLABLE W/O TEMP S7 CONN (Electrode: METTLER TOLEDO, pH Sensor LE 420)



\*The electrode (picture attached below) should be compatible with the Steroglass Flash automatic titrator.



1. ACCESSORY: S7/BNC CABLE FOR PH ELECTRODES