{"text_format":"3","workbook":"xls","n_sheets":9,"sheets":["XXXX","BUILDING COST SUMMARY","PROFFESSIONAL FEES","PRELIM&GENERAL","MAKHUDUTHAMAGA OFFICE","KGAOLA MAFIRI OFFICE BLOCK","COMMUNITY SERVICES OFFICES","NEBO TESTING CENTER","SEKHUKHUNE TESTING CENTER"],"not_rendered":{"external_links":1,"defined_names":22},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"XXXX","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"BUILDING COST SUMMARY","index":1,"n_rows":34,"n_cols":12,"rows_kept":34,"merged":[[4,1,4,2],[9,1,9,5],[10,1,10,5],[11,1,11,5],[12,1,12,5],[13,1,13,5],[14,1,14,5],[15,1,15,4],[17,1,17,4],[21,2,21,9],[22,2,22,9],[23,2,23,9],[24,2,24,9],[25,2,25,9],[26,2,26,9],[27,2,27,9],[28,2,28,3]],"flags":["formulas_cached_only"]}
[]
[null,"PREPARED FOR:","MUKHUDUTHAMAGA OFFICE BUILDINGS"]
[]
[null,"FIRE SERVICES BILL OF QUANTITIES"]
[null,"FIRE SERVICE BILL ACCORDING TO DRAWINGS "]
[]
[]
[null,"Item","Element",{"$nulls":6},"Amount"]
[]
[null,"Preliminaries and General Items"]
[null,"MAKHUDUTHAMAGA MAIN OFFICE",{"$nulls":4},"Sum"]
[null,"KGAOLA MAFIRI OFFICE BLOCK",{"$nulls":4},"Sum"]
[null,"COMMUNITY SERVICES OFFICES",{"$nulls":4},"Sum"]
[null,"NEBO TESTING CENTER",{"$nulls":4},"Sum"]
[null,"SEKHUKHUNE TESTING CENTER",{"$nulls":4},"Sum"]
[null,"SUB-TOTAL EXCLUDING 15% VAT"]
[null,"VALUE ADD TAX"]
[null,"TOTAL AMOUNT INCLUDING 15% VAT "]
[{"$nulls":11},0]
[null,null,"Qualifications:"]
[]
[null,"1","This Bill of Quantities forms part of the contract documents and is to be read in conjunction therewith."]
[null,"2","All works billed here shall include for the full scope of service specified including but not limited to supply, delivery, installation, commissioning, documentation, building tuning, project closeout and administrative requirements, and all works as necessary to provide a working product in accordance with the project performance criteria."]
[null,"3","Quantities indicated here are to be verified by the contractor against the project drawings.  All discrepancies shall be brought to the attention of the responsible engineer.  Should no queries be raised the contract totals and rates provided shall be deemed sufficient for the due execution of the works in accordance with the engineers intent communicated through the project drawings and these specifications."]
[null,"4","No variation in rates shall be due based on variation in quantities, rate of exchange or escalation."]
[null,"5","Errors and omissions of equipment or material required to execute the project solution specified or indicated on the drawings shall be brought to the attention of the responsible engineer for clarification, failing which the provision of such items shall be deemed included in the project rates."]
[null,"6","All works required to execute the scope of works in accordance with the project program and quality requirements are deemed included in the rates and totals provided below."]
[null,"7","Rates provided shall include for fixing, hangers, fittings, transformations, sealant and all other items required to deliver a functional system in accordance with the design intent and specifications. Rate includes the supply,delivery,labour and installation of equipment"]
[null,"8","The bill of quantities shall not be used as the basis for material order."]
[]
[]
[]
[]
[{"$nulls":9},{"v":0,"d":"R 0.00"}]

{"sheet":"PROFFESSIONAL FEES","index":2,"n_rows":71,"n_cols":21,"rows_kept":71,"hidden":true,"merged":[[0,1,0,6],[1,1,1,6],[4,1,4,6],[13,1,13,6],[15,2,15,3],[17,1,17,3],[18,2,18,3],[19,2,19,3],[24,1,24,6],[36,1,36,6],[37,1,37,2],[46,1,46,6],[47,1,47,2],[55,1,55,6],[62,1,62,6]],"flags":["formulas_cached_only"]}
[null,"PROFESSIONAL SERVICES "]
[null,"MAKHUDUTHAMAGA MAIN OFFICE BUILDING"]
[]
[]
[null,"ESTIMATED CONSTRUCTION COSTS"]
[]
[{"$nulls":17},{"v":0,"d":"R 0.00"},{"v":1,"d":"100%"},null,{"v":0,"d":"R0.00"}]
[null,"Total construction cost",{"$nulls":3},"Estimate",{"v":0,"d":"R 0.00"},{"$nulls":10},"X",{"v":0.08,"d":"8%"},null,{"v":0,"d":"R0.00"}]
[]
[{"$nulls":6},{"v":0,"d":"R 0.00"}]
[]
[null,"TOTAL ESTIMATED CONSTRUCTION COSTS",{"$nulls":3},"(Excl. VAT)",{"v":0,"d":"R 0.00"}]
[]
[null,"FEE CALCULATION "]
[]
[null,"Description",{"$nulls":3},"Percentage Fee","Amount"]
[]
[null,"Basic Fees",{"$nulls":3},{"v":0.08,"d":"8.00%"},{"v":0,"d":"R 0.00"},{"$error":"#DIV/0!"},{"$nulls":6},0,null,{"v":0,"d":"R0.00"}]
[]
[]
[]
[null,"A) BASIC FEE",{"$nulls":4},{"v":0,"d":"R 0.00"},{"$nulls":9},17391303]
[]
[{"$nulls":16},19999998.45]
[null,"PROGRESS PAYMENT CERTIFICATE"]
[null,"Stage of services",null,"% points",null,"Progress per stage"]
[{"$nulls":3},"per stage","Fees per stage","%"]
[null,"Preliminary Design",null,30,{"v":0,"d":"R 0.00"},{"v":0,"d":"0%"},{"v":0,"d":"R 0.00"}]
[null,"Design and Tender",null,30,{"v":0,"d":"R 0.00"},{"v":0,"d":"0%"},{"v":0,"d":"R 0.00"},{"$nulls":5},{"v":229011483.25,"d":"229,011,483.25"}]
[null,"Working Drawings ",null,15,{"v":0,"d":"R 0.00"},{"v":0,"d":"0%"},{"v":0,"d":"R 0.00"}]
[null,"Construction",null,20,{"v":0,"d":"R 0.00"},{"v":0,"d":"0%"},{"v":0,"d":"R 0.00"}]
[null,"Close Out",null,5,{"v":0,"d":"R 0.00"},{"v":0,"d":"0%"},{"v":0,"d":"R 0.00"},{"$nulls":5},{"v":0.0707,"d":"7.07%"}]
[null,"Sub-Total",null,100,{"v":0,"d":"R 0.00"}]
[null,"PROGRESS FEE TO DATE",null,null,"(Excl. VAT)",null,{"v":0,"d":"R 0.00"},{"$nulls":5},16191111.865775]
[]
[]
[null,"REIMBURSABLE FEES FOR SPECIALIST SERVICES"]
[null,"Description"]
[]
[null,"A.) Survey",{"$nulls":3},"Estimate (Excl VAT)",{"v":18000,"d":"R 18,000.00"}]
[null,"B.) Geotechnical Investigations",{"$nulls":3},"Estimate (Excl VAT)",{"v":25000,"d":"R 25,000.00"}]
[null,"C.) Occupational Health & Safety (OHS)",{"$nulls":3},"Estimate (Excl VAT)",{"v":45000,"d":"R 45,000.00"}]
[null,"F.) Mark-up for Specialist Services",{"$nulls":3},"10% (ten Percentage)",{"v":7000,"d":"R 7,000.00"}]
[null,"B.) SUB-TOTAL FOR REIMBURSABLE EXPENDITURE SPECIALIST SERVICES",{"$nulls":4},{"v":77000,"d":"R 77,000.00"}]
[]
[]
[null,"REIMBURSABLE EXPENDITURE  FOR PROFESSIONAL SERVICES"]
[null,"Description"]
[null,"A.) Construction Supervision ",{"$nulls":3},"Estimate (Excl VAT)",{"v":270000,"d":"R 270,000.00"}]
[null,"B.) Disbursements ",{"$nulls":5},16950]
[null,"     B.1) Printing and Copying",{"$nulls":3},"Estimate (Excl VAT)",{"v":35000,"d":"R 35,000.00"},{"$nulls":5},{"v":408600,"d":"R 408,600.00"}]
[null,"     B.2) Travelling ",{"$nulls":3},"Estimate (Excl VAT)",{"v":26600,"d":"R 26,600.00"},{"v":1477.7777777777778,"d":"R 1,477.78"}]
[{"$nulls":7},{"v":0,"d":"R 0.00"}]
[null,"C.) SUB-TOTAL FOR REIMBURSABLE EXPENDITURES",{"$nulls":4},{"v":331600,"d":"R 331,600.00"},5911.111111111111]
[]
[null,"TOTAL PROJECT PROFESSIONAL FEE BUDGET"]
[]
[null,"Sub Total (A + B + C)",{"$nulls":4},{"v":408600,"d":"R 408,600.00"},{"$nulls":5},{"v":57204.00000000001,"d":"R 57,204.00"}]
[]
[null,"GRAND TOTAL",{"$nulls":4},{"v":408600,"d":"R 408,600.00"}]
[]
[]
[null,"TOTAL PROJECT  BUDGET"]
[]
[null,"Construction",{"$nulls":4},{"v":0,"d":"R 0.00"}]
[]
[null,"Professional Fees",{"$nulls":4},{"v":408600,"d":"R 408,600.00"}]
[]
[null,"VAT @ 15%",{"$nulls":4},{"v":61290,"d":"R 61,290.00"}]
[]
[null,"GRAND TOTAL",{"$nulls":4},{"v":469890,"d":"R 469,890.00"}]

{"sheet":"PRELIM&GENERAL","index":3,"n_rows":73,"n_cols":6,"rows_kept":73,"merged":[[2,1,2,4]],"flags":["formulas_cached_only"]}
[]
[]
[null,"FIRE SERVICES BILL OF QUANTITIES"]
[]
[null,"PRELIMINARIES AND GENERAL:","ENTIRE FACILITY"]
[]
[null,"BUILDING AREA:","N/A","m2"]
[]
[]
[{"$nulls":4},"SUPPLY","TOTAL"]
["ITEM","ITEM DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT"]
[{"$nulls":4},"AMOUNT"]
[]
[1,"Fixed Obligation (Site Establishment)","Sum",1]
[]
[]
[2,"Health and Safety obligation in respect of the ","Sum",1]
[null,"OHS Act and Construction Regulations"]
[null,"including Covid 19 Complience"]
[]
[]
[4,"Time Related Obligations","Month",3]
[]
[{"v":5,"d":"5.0"},"Protection, removal,relocation and replacement of "]
[null,"Utility services."]
[]
[null,"(a) Utility services"]
[]
[null,"    (i)  Protection, removal,relocation and replacement of utility services","PC Sum",1]
[null,"   (ii)  Handling costs and profit in respect of sub-items (a) (i) above","%",{"v":0,"d":"R 0.00"}]
[]
[null,"Existing  services"]
[]
[null,"Excavate by hand in soft material to expose ","m3",250]
[null,"existing services"]
[]
[null,"Temporarily protection of existing service","Sum"]
[]
[null,"Contractor's charge on  item  A4.2.2","%",{"v":0,"d":"R 0.00"}]
[]
[null,"Relocation of existing services","PC Sum"]
[]
[null,"Contractor's charges on item A4.2.6","%",{"v":0,"d":"R 0.00"}]
[6,"SUM RESERVED FOR PROFFESIONAL FEES",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[null,"Design and Construction supervision","Sum",1,{"v":470000,"d":"R 470,000.00"},{"v":470000,"d":"R 470,000.00"}]
[]
[7,"OPERATING AND MAINTENANCE MANUALS",""]
[null,"The Contractor shall make provision for 4 x copies of O & M Manuals in accordance with the detail in the Standard specification.","No",0]
[]
[8,"TRAINING OF CLIENTS STAFF",""]
[null,"The Contractor shall make provision for 1 full day's training of the Clients Staff, on the operation of the installation.","Sum",1]
[]
[9,"Additional test required",""]
[null,"Geotechnical","Sum",1,{"v":120000,"d":"R 120,000.00"},{"v":120000,"d":"R 120,000.00"}]
[null,"Survey","Sum",1,{"v":110000,"d":"R 110,000.00"},{"v":110000,"d":"R 110,000.00"}]
[]
[10,"COMMISIONING AND TESTING",""]
[]
[10.1,"MAINTENANCE AND GUARANTEE",""]
[]
[10.2,"The Contractor shall make provision for 1 x Full years Maintenance and Guarantee of the entire installation. 11 x Standard Maintenance visits and 1 x Major service is required throughout the 12 months.","lot",1]
[]
[10.3,"Fire Signage as indicated in the drawings issued","Sum"]
[]
[]
[]
[]
[null,"SUB-TOTAL AMOUNTS"]
[]
[]
[]
[]
[{"$nulls":5},{"v":0,"d":"R 0.00"}]

{"sheet":"MAKHUDUTHAMAGA OFFICE","index":4,"n_rows":122,"n_cols":6,"rows_kept":122,"merged":[[2,1,2,4]],"flags":["formulas_cached_only"]}
[]
[]
[null,"CONSTRUCTION OF AN EMERGENCY EXIT IN THE MAIN BUILDING BILL OF QUANTITIES"]
[null,"STRUCTURE:","MAKHUDUTHAMAGA MAIN OFFICE"]
[]
[null,"BUILDING AREA:",null,"m2"]
[]
[]
["ITEM","ITEM DESCRIPTION","UNIT","QUANTITY","RATE","TOTAL"]
[{"$nulls":4},"AMOUNT","AMOUNT"]
[]
[1,"GROUND FLOOR"]
[]
[null,"Supply and install  fire protection equipment as specified and indicated on the drawings."]
[1.1,"Fire Protection Equipment"]
["1,1,1","4.5Kg DCP Fire Extinguishers","No.",11]
["1,1,2","F13 Signage 190mm x 190mm","No.",8]
["1,1,3","F15 Signage 190mm x 190mm","No.",3]
["1,1,4","F4 Signage 190mm x 190mm","No.",3]
["1,1,5","E6 Signage 290mm x 290mm","No.",5]
["1,1,6","E1 Signage 290mm x 290mm","No.",4]
["1,1,7","E2 Signage 290mm x 290mm","No.",4]
["1,1,8","E3 Signage 290mm x 290mm","No.",13]
[]
[2,"FIRST FLOOR"]
[null,"Supply and install  fire protection equipment as specified and indicated on the drawings."]
[]
[2.1,"Fire Protection Equipment"]
["2.1.1","4.5Kg DCP Fire Extinguishers","No.",10]
["2.1.2","F13 Signage 190mm x 190mm","No.",10]
["2.1.3","E1 Signage 290mm x 290mm","No.",2]
["2.1.4","E2 Signage 290mm x 290mm","No.",2]
["2.1.5","E3 Signage 290mm x 290mm","No.",8]
["2.1.6","E18 Signage 290mm x 290mm","No.",1]
[]
[]
[3,"SITE"]
[]
["3.1","DEMOLISHING"]
[]
[null,"Demolish and remove structures / buildings","No",5]
[]
["3.2","EARTHWORKS (PIPE TRENCHES)"]
[]
["3.2.1","TRENCHES FOR WATER PIPES"]
[]
[null,"Excavate in all materials for trenches, backfill, compose"]
[null,"and dispose of surplus/unsuitable material for water "]
[null,"pipes to the following depths:"]
[null,"(Note: Freehaul distance is 2.0km)"]
[]
[null,"(a) Pipes over 0m and up to 2.0m (800mm wide trench):"]
[null,"(a)75 mm dia","m",36]
[null,"(b)90 mm dia","m",800]
[null,"(c)110mm dia","m",18]
[]
["3.2.2","Extra over item 4.1 above for:"]
[null,"Intermediate excavation  ","m³",576]
[null,"Hard rock excavation     ","m³",{"v":172.79999999999998,"d":"173"}]
[]
["3..2.3","Remove and store block or brick paving","m2",50]
[]
["3.2.4","Cutting of existing concrete paving","m",50]
[]
["3.2.5","Breaking out of existing concrete paving and dispose","m2",50]
[]
[]
[null,"TOTAL CARRIED FORWARD"]
[]
[]
[null,"TOTAL BROUGHT FORWARD"]
[]
["3.3","FINISHING"]
[]
[]
["3.3.1","Reinstate paving with stored paving"]
[]
[null,"a) Interlocking concrete block paving","m2",50]
[]
["3.3.2","Reinstate concrete (Class 20 Mpa) paving up to"]
[null,"100mm thick"]
[]
[null,"a) Wood float finish","m2",50]
[]
[null,"b) Steel float finish","m2",50]
[]
[null,"c) Imprint finish (any pattern)","m2",10]
[]
["3.4","MEDIUM PRESSURE PIPELINES"]
[]
[null,"Supply, lay, bed and test the following uPVC pressure pipes"]
[null,"(conforming with SANS 966-1 specifications) in 6m each pipe"]
[null,"fitted at one end with socket for mechanical jointing: Including bends, in the following diameters (testing measured elsewhere):"]
[]
[null,"i)  Class 12 PVC pipes, SANS 966:1998 Part 1 (uPVC)"]
[null,"(a)75 mm dia","m",36]
[null,"(b)90 mm dia","m",800]
[null,"(c)110mm dia","m",18]
[]
["3.5","SUPPLY & INSTALL FIRE HYDRANT COMPLETE AS PER DRAWING "]
["3.5.1"," 65 mm Pillar Type Fire Hydrant ","No.",3]
["3.5.2","Anchor / thrust blocks class 15 / 19 concrete","m³",3]
["3.5.3","Concrete casing","m³",3]
[]
[]
[]
["3.6","ELEVATED STEEL TANK AND STAND"]
["3.6.1","supply and install 90kl elevated steel tank on a 9m high stand.","Prov Sum",1]
[]
["3.6.2","Contractor's handling charge on Item 9.1.1 and 9.12","%",0]
[]
["3.7","PIPEWORK"]
[null,"Elevated Tank pipework. (as specified and indicated on the drawings)","Sum",1]
[null,"All steel pipes and fittings to have a wall thickness of 4.5mm and to be Galvenised Mild Steel (GMS)"]
[null," "]
["3.8","SUPPLY AND INSTALL FIRE BOOSTER PUMPS","No.","Sum "]
[]
["3.9","CONSTRUCTION OF FIRE EXIT STAIRCASE COMPLETE AS PER DRAWING","No",2]
[]
[]
[]
[null,"SUB-TOTAL AMOUNTS"]

{"sheet":"KGAOLA MAFIRI OFFICE BLOCK","index":5,"n_rows":107,"n_cols":8,"rows_kept":107,"merged":[[2,1,2,4]],"flags":["formulas_cached_only"]}
[]
[]
[null,"FIRE SERVICES BILL OF QUANTITIES"]
[]
[null,"STRUCTURE:","KGAOLA MAFIRI OFFICE BLOCK"]
[null,"DATE:","2023-08-21T14:38:36.910"]
[null,"BUILDING AREA:",null,"m2"]
[]
[]
[{"$nulls":4},"RATE","TOTAL"]
["ITEM","ITEM DESCRIPTION","UNIT","QUANTITY","AMOUNT","AMOUNT"]
[]
[]
[1,"Supply and install  fire protection equipment as specified and indicated on the drawings."]
[]
[1.1,"Fire Protection Equipment"]
["1,1,1","4.5Kg DCP Fire Extinguishers","No.",12,{"$nulls":3},942.5]
["1,1,2","F13 Signage 190mm x 190mm","No.",8]
["1,1,3","F15 Signage 190mm x 190mm","No.",3]
["1,1,4","F4 Signage 190mm x 190mm","No.",4]
["1,1,5","E6 Signage 290mm x 290mm","No.",1]
["1,1,6","E1 Signage 290mm x 290mm","No.",4]
["1,1,7","E2 Signage 290mm x 290mm","No.",3]
["1,1,8","E3 Signage 290mm x 290mm","No.",9]
[]
[]
[2,"Site "]
[]
["2.2","EARTHWORKS (PIPE TRENCHES)"]
[]
["3.2.1","TRENCHES FOR WATER PIPES"]
[]
[null,"Excavate in all materials for trenches, backfill, compose"]
[null,"and dispose of surplus/unsuitable material for water "]
[null,"pipes to the following depths:"]
[null,"(Note: Freehaul distance is 2.0km)"]
[]
[null,"(a) Pipes over 0m and up to 2.0m (800mm wide trench):"]
[null,"(a)75 mm dia","m",15]
[null,"(b)90 mm dia","m",450]
[null,"(c)110mm dia","m",30]
[]
["3.2.2","Extra over item 4.1 above for:"]
[null,"Intermediate excavation  ","m³",576]
[null,"Hard rock excavation     ","m³",144]
[]
["3..2.3","Remove and store block or brick paving","m2",50]
[]
["3.2.4","Cutting of existing concrete paving/asphalt paving","m",50]
[]
["3.2.5","Breaking out of existing concrete paving and dispose","m2",50]
[]
["3.3","FINISHING"]
[]
[]
["3.3.1","Reinstate paving with stored paving"]
[]
[null,"a) Interlocking concrete block paving","m2",50]
[]
[null,"b) 25mm Asphalt","m2",50]
[]
[]
["3.3.2","Reinstate concrete (Class 20 Mpa) paving up to"]
[null,"100mm thick"]
[]
[null,"a) Wood float finish","m2",50]
[]
[null,"b) Steel float finish","m2",50]
[]
[null,"c) Imprint finish (any pattern)","m2",10]
[]
["3.4","MEDIUM PRESSURE PIPELINES"]
[]
[null,"Supply, lay, bed and test the following uPVC pressure pipes"]
[null,"(conforming with SANS 966-1 specifications) in 6m each pipe"]
[null,"fitted at one end with socket for mechanical jointing: Including bends, in the following diameters (testing measured elsewhere):"]
[]
[null,"i)  Class 12 PVC pipes, SANS 966:1998 Part 1 (uPVC)"]
[null,"(a)75 mm dia","m",15]
[null,"(b)90 mm dia","m",450]
[null,"(c)110mm dia","m",30]
[]
["3.5","SUPPLY & INSTALL FIRE HYDRANT COMPLETE AS PER DRAWING "]
["3.5.1"," 65 mm Pillar Type Fire Hydrant ","No.",2]
["3.5.2","Anchor / thrust blocks class 15 / 19 concrete","m³",3]
["3.5.3","Concrete casing","m³",3]
[]
[]
[]
["3.6","ELEVATED STEEL TANK AND STAND"]
["3.6.1","supply and install 90kl elevated steel tank on a 9m high stand.","Prov Sum",1]
[]
["3.6.2","Contractor's handling charge on Item 9.1.1 and 9.12","%",0]
[]
["3.7","PIPEWORK"]
[null,"Elevated Tank pipework. (as specified and indicated on the drawings)","Sum",1]
[null,"All steel pipes and fittings to have a wall thickness of 4.5mm and to be Galvenised Mild Steel (GMS)"]
[null," "]
["3.8","SUPPLY AND INSTALL FIRE BOOSTER PUMPS","No.","Sum "]
{"$rows_empty":7}
[null,"SUB-TOTAL AMOUNTS"]

{"sheet":"COMMUNITY SERVICES OFFICES","index":6,"n_rows":45,"n_cols":6,"rows_kept":45,"merged":[[2,1,2,4]],"flags":["formulas_cached_only"]}
[]
[]
[null,"FIRE SERVICES BILL OF QUANTITIES"]
[]
[null,"STRUCTURE:","COMMUNITY SERVICES OFFICES"]
[null,"DATE:","2023-08-21T14:38:36.910"]
[null,"BUILDING AREA:",null,"m2"]
[]
[]
[{"$nulls":4},"RATE","TOTAL"]
["ITEM","ITEM DESCRIPTION","UNIT","QUANTITY","AMOUNT","AMOUNT"]
[]
[]
[1]
[]
[1.1,"Fire Protection Equipment"]
["1,1,1","4.5Kg DCP Fire Extinguishers","No.",3]
["1,1,2","F13 Signage 190mm x 190mm","No.",3]
["1,1,3","E6 Signage 290mm x 290mm","No.",3]
["1,1,4","E1 Signage 290mm x 290mm","No.",1]
["1,1,5","E2 Signage 290mm x 290mm","No.",1]
["1,1,6","E3 Signage 290mm x 290mm","No.",5]
{"$rows_empty":22}
[null,"SUB-TOTAL AMOUNTS"]

{"sheet":"NEBO TESTING CENTER","index":7,"n_rows":45,"n_cols":6,"rows_kept":45,"merged":[[2,1,2,4]],"flags":["formulas_cached_only"]}
[]
[]
[null,"FIRE SERVICES BILL OF QUANTITIES"]
[]
[null,"STRUCTURE:","NEBO TESTING CENTER"]
[null,"DATE:","2023-08-21T14:38:36.910"]
[null,"BUILDING AREA:",null,"m2"]
[]
[]
[{"$nulls":4},"RATE","TOTAL"]
["ITEM","ITEM DESCRIPTION","UNIT","QUANTITY","AMOUNT","AMOUNT"]
[]
[]
[1,"TESTING CENTER"]
[]
[1.1,"Fire Protection Equipment"]
["1,1,1","4.5Kg DCP Fire Extinguishers","No.",2]
["1,1,2","F13 Signage 190mm x 190mm","No.",2]
["1,1,3","E6 Signage 290mm x 290mm","No.",1]
["1,1,4","E3 Signage 290mm x 290mm","No.",1]
[]
[2,"GUARD HOUSE"]
[]
[2.1,"Fire Protection Equipment"]
["2.1.1","4.5Kg DCP Fire Extinguishers","No.",1]
["2.1.2","F13 Signage 190mm x 190mm","No.",1]
["2.1.3","E3 Signage 290mm x 290mm","No.",1]
[]
[3,"OFFICE"]
[]
[3.1,"Fire Protection Equipment"]
["3.1.1","4.5Kg DCP Fire Extinguishers","No.",2]
["3.1.2","F13 Signage 190mm x 190mm","No.",2]
["3.1.3","E6 Signage 290mm x 290mm","No.",2]
["3.1.4","E3 Signage 290mm x 290mm","No.",2]
{"$rows_empty":9}
[null,"SUB-TOTAL AMOUNTS"]

{"sheet":"SEKHUKHUNE TESTING CENTER","index":8,"n_rows":48,"n_cols":6,"rows_kept":48,"merged":[[2,1,2,4]],"flags":["formulas_cached_only"]}
[]
[]
[null,"FIRE SERVICES BILL OF QUANTITIES"]
[]
[null,"STRUCTURE:","SEKHUKHUNE TESTING CENTER"]
[null,"DATE:","2023-08-21T14:38:36.910"]
[null,"BUILDING AREA:",null,"m2"]
[]
[]
[{"$nulls":4},"RATE","TOTAL"]
["ITEM","ITEM DESCRIPTION","UNIT","QUANTITY","AMOUNT","AMOUNT"]
[]
[]
[1,"TESTING CENTER"]
[]
[1.1,"Fire Protection Equipment"]
["1,1,1","4.5Kg DCP Fire Extinguishers","No.",1]
["1,1,2","F13 Signage 190mm x 190mm","No.",1]
["1,1,3","E3 Signage 290mm x 290mm","No.",1]
["1,1,4","E6 Signage 290mm x 290mm","No.",1]
[]
[2,"GUARD HOUSE"]
[]
[2.1,"Fire Protection Equipment"]
["2.1.1","4.5Kg DCP Fire Extinguishers","No.",1]
["2.1.2","F13 Signage 190mm x 190mm","No.",1]
["2.1.3","E3 Signage 290mm x 290mm","No.",1]
[]
[3,"CENTER OFFICE"]
[]
[3.1,"Fire Protection Equipment"]
["3.1.1","4.5Kg DCP Fire Extinguishers","No.",1]
["3.1.2","F13 Signage 190mm x 190mm","No.",1]
["3.1.3","E3 Signage 290mm x 290mm","No.",1]
["3.1.4","E6 Signage 290mm x 290mm","No.",1]
{"$rows_empty":12}
[null,"SUB-TOTAL AMOUNTS"]