{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["A&B Schedules","Deviation Schedule","Test Schedule"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"A&B Schedules","index":0,"n_rows":68,"n_cols":9,"rows_kept":68,"merged":[[1,1,1,6],[2,1,2,6],[3,1,3,6],[4,1,4,6],[7,2,7,3],[8,2,8,3],[9,3,9,4],[19,3,19,4],[24,3,24,4],[30,3,30,4],[35,2,35,4],[36,2,36,4],[37,3,37,4],[42,3,42,4],[58,1,58,6],[60,0,60,6],[62,0,62,1],[67,2,67,3]]}
[{"$nulls":3},"ESKOM TENDER E2719DXLIMOU"]
[null,"Technical Schedules A and B for"]
[null,"CLAMP,STRAIN3B STWIRE;70 KN;16-5 MM D-DT-7022"]
[null,"Schedule A:  Purchasers specific requirements"]
[null,"Schedule B:  Guarantees and technical particulars of equipment offered"]
[]
[null,1,null,2,null,3,4]
[null,"Item ","Description",null,null,"Schedule A","Schedule B"]
[null,1,"Product Information"]
[null,1.1,"·","Purchasing details"]
[null,"1.1.1",null,"Eskom SAP No",null,{"v":401307,"d":"0401307"},"xxxxxxxxxx"]
[null,"1.1.2",null,"Manufacturer","Manufacturer Name","xxxxxxxxxx"]
[null,"1.1.3",null,"Manufacturer's Product Code","Product Code","xxxxxxxxxx"]
[null,"1.1.4",null,"Manufacturer's Drawing number & Revision number","Drawing and Revision Number","xxxxxxxxxx"]
[null,"1.1.5",null,"Manufacturer's physical identification mark on product","Identification Mark","xxxxxxxxxx"]
[null,"1.1.6",null,"Compliance to all dimensions on Eskom Buyer's Guide Drawings   ","Eskom D-DT-7022","YES"]
[null,"1.1.7",null,"Item sample required","OEM Only","YES","xxxxxxxxxx"]
[null,"1.1.8",null,"Item supplied with:\n1 X M16 X 75mm Clevis Bolt Assembly (D-DT-7043),\n\n3 X Galvanised Steel 12mm U-Bolts with 6 X Spring Washers (D-DT-3014),\n\n6 X M12 Hexagon Nut (D-DT-3173), and Malleable Iron Keeper;","Eskom D-DT-7022","YES",null,null,"CoE Query"]
[]
[null,1.2,"·","Mechanical Properties"]
[null,"1.2.1",null,"Mechanical failing load","kN",70]
[null,"1.2.2",null,"Material Grade (Body and Keeper)",null,"Malleable Cast Iron"]
[null,"1.2.3",null,"Cast/Moulding Lines removed on inside of clamp",null,"YES"]
[]
[null,1.3,"·","Coupling interfaces (where applicable)"]
[null,"1.3.1",null,"1st Coupling Type on fitting","16L Clevis","YES"]
[null,"1.3.2",null,"Coupling orientation as per DDT Drawing","Eskom D-DT-7022","YES"]
[null,"1.3.3",null,"Conductor range","mm","5,0 - 16,0"]
[null,"1.3.4",null,"Hump back pin in accordance with Eskom 240-75883164",null,"YES"]
[]
[null,1.4,"·","Galvanising (where applicable)"]
[null,"1.4.1",null,"Average minimum galvanising thickness on product body and keeper complies to SANS 121",null,"YES"]
[null,"1.4.2",null,"Average minimum galvanising thickness on clevis bolt complies to SANS 121",null,"YES"]
[null,"1.4.3",null,"Average minimum galvanising thickness on steel U-bolts complies to SANS 121",null,"YES"]
[]
[null,2,"Documentation (to be submitted with tender)"]
[null,null,"Note:  All documentation to also be provided in electronic format."]
[null,2.1,"·","General"]
[null,"2.1.1",null,"Approved Manufacturer Drawings showing markings and dimensions","1 Set submitted","YES"]
[null,"2.1.2",null,"Material grade certification","Certification submitted","YES"]
[null,"2.1.3",null,"Visual inspection of welds according to Eskom 240-75883830 (where applicable)","As per Eskom 240-75883830","YES or N/A"]
[]
[null,2.2,"·","Test Reports (where applicable)",null,"Required","Report\nNumber"]
[null,"2.2.1",null,"Visual examination (SANS 61284)","Test Report Submitted","Report number"]
[null,"2.2.2",null,"Dimensional and material verification (SANS 61284)","Test Report Submitted","Report number"]
[null,"2.2.3",null,"Hot Dip Galvanising certificate for body and keeper (SANS 61284)","Test Report Submitted","Report number"]
[null,"2.2.4",null,"Hot Dip Galvanising certificate for clevis bolt assembly (SANS 61284)","Test Report Submitted","Report number"]
[null,"2.2.5",null,"Hot Dip Galvanising certificate for U-bolt assembly (SANS 61284)","Test Report Submitted","Report number"]
[null,"2.2.6",null,"Verification of Clevis (SANS 60471)","Test Report Submitted","Report number"]
[null,"2.2.7",null,"Non-destructive testing - Hardness Test  (SANS 61284)","Test Report Submitted","Report number",null,null,"CoE Query"]
[null,"2.2.8"]
[null,"2.2.9",null,"Mechanical Tests (where applicable)",null,"Required","Report\nNumber"]
[null,"2.2.10",null,"Damage and failure load test (SANS 61284)","Test Report Submitted","Report number"]
[null,"2.2.11",null,"Clamp bolt tightening test (SANS 61284)","Test Report Submitted","Report number"]
[null,"2.2.12",null,"Tensile test (SANS 61284)","Test Report Submitted","Report number"]
[null,"2.2.13",null,"Damage and failure load test of the attachment point used during erection (SANS 61284)","Test Report Submitted","Report number"]
[null,"2.2.14",null,"Hump back split pin pull test (Eskom 240-75883164)","Test Report Submitted","Report number"]
[]
[null,"NOTE:  DEVIATION SCHEDULE CONTINUE ON NEXT PAGE.\n             IF NO DEVIATIONS ARE MENTIONED ON THE DEVIATION SCHEDULE IT WILL BE ACCEPTED\n             THAT THE SUPPLIER AND MANUFACTURER FULLY COMPLIES WITH THE REQUIREMENTS OF\n             THE ESKOM SPECIFICATON(S)."]
[{"$nulls":3},"ESKOM TENDER E2719DXLIMOU"]
["SUPPLIER SIGNATURES"]
[]
[null,null,"         "]
[{"$nulls":3},"Name (Print)",null,null,"Company Name"]
[]
[]
[]
[null,null,"Sign",{"$nulls":3},"Date"]

{"sheet":"Deviation Schedule","index":1,"n_rows":45,"n_cols":6,"rows_kept":45,"merged":[[0,0,0,6],[1,0,1,6],[2,0,2,1],[3,0,3,6],[4,2,4,6],[5,2,5,6],[6,2,6,6],[7,2,7,6],[8,2,8,6],[9,2,9,6],[10,2,10,6],[11,2,11,6],[12,2,12,6],[13,2,13,6],[14,2,14,6],[15,2,15,6],[16,2,16,6],[17,2,17,6],[18,2,18,6],[19,2,19,6],[20,2,20,6],[21,2,21,6],[22,2,22,6],[23,2,23,6],[24,2,24,6],[25,2,25,6],[26,2,26,6],[27,2,27,6],[28,2,28,6],[29,2,29,6],[30,2,30,6],[31,2,31,6],[32,2,32,6],[33,2,33,6],[34,2,34,6],[37,1,37,6],[40,1,40,3],[40,5,40,6],[44,1,44,3],[44,5,44,6]]}
["ESKOM TENDER E2719DXLIMOU"]
["Deviation schedule"]
["SAP 401307"]
["Any deviations offered to this specification shall be listed below with reasons for deviation.  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective that that specified by Eskom."]
["Item","Clause","Description of Deviation"]
{"$rows_empty":30}
["SIGNATURES"]
[]
[null,"SUPPLIER SIGNATURES"]
[]
[null,"         "]
[null,"Name (Print)",{"$nulls":3},"Company Name"]
[]
[]
[]
[null,"Sign",{"$nulls":3},"Date"]

{"sheet":"Test Schedule","index":2,"n_rows":30,"n_cols":5,"rows_kept":30,"merged":[[1,1,1,4],[2,1,2,4],[3,1,3,4],[19,1,19,2],[22,0,22,5],[25,0,25,2],[25,4,25,5],[29,0,29,2],[29,4,29,5]]}
[null,null,"ESKOM TENDER E2719DXLIMOU"]
[null,"Test Report Schedule"]
[null,"CLAMP,STRAIN3B STWIRE;70 KN;16-5 MM"]
[null,"SAP 401307"]
[null,1,2,3,4]
[null,"Item ","Description","Specification","Report No."]
[null,"2.2.1","Visual examination","SANS 61284"]
[null,"2.2.2","Dimensional and material verification","SANS 61284"]
[null,"2.2.3","Hot Dip Galvanising certificate for body and keeper","SANS 61284"]
[null,"2.2.4","Hot Dip Galvanising certificate for clevis bolt assembly","SANS 61284"]
[null,"2.2.5","Hot Dip Galvanising certificate for U-bolt assembly","SANS 61284"]
[null,"2.2.6","Verification of Clevis","SANS 60471"]
[null,"2.2.7","Non-destructive testing - Hardness Test","SANS 61284"]
[null,"2.2.8","Damage and failure load test","SANS 61284"]
[null,"2.2.9","Clamp bolt tightening test","SANS 61284"]
[null,"2.2.10","Tensile test","SANS 61284"]
[null,"2.2.11","Damage and failure load test of the attachment point used during erection ","SANS 61284"]
[null,"2.2.12","Hump back split pin pull test","Eskom 240-75883164"]
[]
[]
[]
[]
["SUPPLIER SIGNATURES"]
[]
["         "]
["Name (Print)",{"$nulls":3},"Company Name"]
[]
[]
[]
["Sign",{"$nulls":3},"Date"]