{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["DBSA01"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"DBSA01","index":0,"n_rows":1349,"n_cols":7,"rows_kept":1349}
["ITEM NO","DESCRIPTION",null,"UNIT","QUANTITY","RATE","AMOUNT"]
[null,"BILL NO. 1",null,"H1",0]
[]
[null,"PRELIMINARIES",null,"H1",0]
[]
[null,"BUILDING AGREEMENT AND PRELIMINARIES",null,"H1",0]
[]
[null,"The JBCC Series 2000 Principal Building Agreement (March 2005 edition) prepared by the Joint Building Contract Committee shall be the applicable building agreement, amended as hereinafter described ",null,null,0]
[]
[null,"The ASAQS Preliminaries (March 2005 edition) published by the Association of South African Quantity Surveyors for use with the said JBCC Principal Building Agreement shall be deemed to be incorporated in these bills of quantities. ",null,null,0]
[]
[null,"Contractors are referred to the above mentioned documents for the full intent and meaning of each clause thereof. ",null,null,0]
[]
[null,"These clauses are hereinafter referred to by clause number and heading only. Where standard clauses or alternatives are not entirely applicable to this contract such modifications, corrections or supplements as will apply are given under each relevant clause heading and such modifications, corrections or supplements shall take precedence notwithstanding anything contrary contained in the above mentioned documents. ",null,null,0]
[]
[null,"Where any item is not relevant to this specific contract such item is marked N/A, signifying \"not applicable\" ",null,null,0]
[]
[null,"PREAMBLES FOR TRADES  ",null,"H2",0]
[]
[null,"The Model Preambles for Trades (2008 edition) as published by the Association of South African Quantity Surveyors shall be deemed to be incorporated in these bills of quantities and no claims arising from brevity of description of items fully described in the said Model Preambles will be entertained ",null,null,0]
[]
[null,"Supplementary preambles are incorporated in these bills of quantities to satisfy the requirements of this project. Such supplementary preambles shall take precedence over the provisions of the said Model Preambles. ",null,null,0]
[]
[null,"The contractor's prices for all items throughout these bills of quantities must take account of and include for all of the obligations, requirements and specifications given in the said Model Preambles and in any supplementary  preambles  ",null,null,0]
[]
[null,"PRICING OF PRELIMINARIES  ",null,"H1",0]
[]
[null,"SECTION A - PRINCIPAL BUILDING AGREEMENT",null,"H1",0]
[]
[null,"Should the contractor select Option A in terms of sub clause 3.2.1 in the Contract Data - Contractor to Employer (CE) for the purpose of adjustment of these preliminaries, the amount entered into the amount column in these preliminaries is to be divided into one or more of the three categories provided namely Fixed (F), Value Related (V) and Time Related (T). ",null,null,0]
[]
[null,"Definitions ",null,null,0]
[]
[1,"Clause 1.0 - Definitions and interpretation  F:..................... V:...................... T:......................... ",null,"Item",0]
[]
[null,"Objective and preparations   ",null,null,0]
[]
[2,"Clause 2.0 - Offer acceptance and performance obligations F:....................... V:........................ T:...................... ",null,"Item",0]
[]
[3,"Clause 4.0 - Design responsibility F:......................... V:...................... T:..................... ",null,"Item",0]
[]
[4,"Clause 5.0 - Employer's agents  F:......................V:..................... T:...................... ",null,"Item",0]
[]
[5,"Clause 6.0 - Contractor's site representative F:....................... V:................... T:.................... ",null,"Item",0]
[]
[6,"Clause 7.0 - Compliance with laws and regulations F:....................... V:.................. T:....................... ",null,"Item",0]
[]
[null,"Without limiting the generality of the provisions of clause 7.0, the contractor's attention is drawn to the provisions of the Construction Regulations, 2003 issued in terms of the Occupational Health and Safety Act, 1993. It is specifically stated that the employer shall prepare a documented health and safety specification for the works and that the employer shall ensure that the contractor has made provision for the cost of health and safety measures during the execution of the works. The contractor shall price opposite this item for compliance with the act and the regulations and the reasonable provisions of the aforementioned health and safety specifications. ",null,null,0]
[]
[null,"The contractor shall allow for and pay any levies required by the National Home Builders Registration Council (NHBRC). The contractor warrants that he is registered and will maintain registration with the NHBRC for the duration of this agreement  F:.................... V:.................... T:............................  ",null,null,0]
[]
[7,"Clause 8.0 - Works risk  F:................. V:..................... T:.................... ",null,"Item",0]
[]
[8,"Clause 9.0 - Indemnities F:....................... V:..................... T:................... ",null,"Item",0]
[]
[9,"Clause 10.0 - General insurances F:................... V:....................T:.................... ",null,"Item",0]
[]
[10,"Clause 11.0 - Special insurances F:..................... V:.................... T:.................. ",null,"Item",0]
[]
[11,"Clause 12.0 - Effecting insurances F:.................. V:..................... T:...................... ",null,"Item",0]
[]
[12,"Clause 13.0 - Assignment  F:......................... V:..................... T:.......................... ",null,"Item",0]
[]
[13,"Clause 14.0 - Security F:.................... V:................... T:.................... ",null,"Item",0]
[]
[null,"Execution  ",null,null,0]
[]
[14,"Clause 15.0 - Preparation for and execution of the works F:................ V:.................. T:..................... ",null,"Item",1]
[]
[15,"Clause 16.0-Site and Access F:................. V:.................. T:....................... ",null,"Item",0]
[]
[16,"Clause 17.0 - Contract instructions  F:................... V:.................... T:..................... ",null,"Item",0]
[]
[17,"Clause 18.0 - Setting out of the works The contractor shall notify the principal agent if any encroachments of adjoining foundations, buildings, structures, pavements, boundaries, etc. exist in order that the necessary arrangements may be made for the rectification of any such encroachments.F:.................. V:......................T:.................. ",null,"Item",0]
[]
[18,"Clause 19.0 - Temporary works and plant   F:.................. V:.................. T:.................... ",null,"Item",0]
[]
[19,"Clause 20.0 - Nominated subcontractors F:................... V:.................... T:.................... ",null,"Item",0]
[]
[20,"Clause 21.0 - Selected subcontractors F:...................... V:.................. T:.................... ",null,"Item",0]
[]
[21,"Clause 22.0 - Employer's direct contractors  F:...................... V:..................... T:...................... ",null,"Item",0]
[]
[22,"Clause 23.0 - Contractor's domestic subcontractors  F:.................. V:................. T:..................... ",null,"Item",0]
[]
[null,"Completion  ",null,null,0]
[]
[23,"Clause 24.0 - Practical completion  F:................. V:.................. T:................... ",null,"Item",0]
[]
[24,"Clause 25.0 - Works Completion25.1.1 The Contractor shall, within (5) working days of receipt of the works completion list, issue a programme indicating the date for completion of the works completion list, for the approval by the principal agent.25.1.2 Should the contractor fail to issue such a programme, it shall be deemed that the contractor agrees to complete the works completion list within (40) working days of the date of receipt of the works completion list.25.1.3 Should the contractor fail to complete the defects and achieve works completion in accordance with the agreed programme or deemed forty (40) day period, and without prejudice to any other rights that the employer might have, the contractor shall be liable to the employer for the penalties as described as the Works Completion Penalty per day until Works Completion is achieved. 25.6 Upon the issue of the certificate of works completion the employer shall be entitled to possession of the works and the site subject to contractor's lien or right of possession of works F:....................... V:.................... T:......................... ",null,"Item",0]
[]
[25,"Clause 26.0 - Final completion F:.................. V:.................. T:................... ",null,"Item",0]
[]
[26,"Clause 27.0 - Latent defects liability period F:.................... V:.................... T:..................... ",null,"Item",0]
[]
[27,"Clause 28.0 - Sectional completion F:..................... V:.................. T:....................... ",null,"Item",0]
[]
[28,"Clause 29.0 - Revision of date for practical completion The removal and replacement of materials and/or workmanship which do not conform to specification or drawing shall not constitute grounds for the extension of the construction period nor for the adjustment of the contract value (Clause 29.3 )  F:......................... V:...................... T:..................... ",null,"Item",0]
[]
[29,"Clause 30.0 - Penalty for late or non-completion  Clause 30.3 - Penalties for not achieving the date of works completion in terms of Clause 25.4 shall be levied at 150% of the penalties defined for not achieving Practical Completion   F:..................... V:................... T:................... ",null,"Item",0]
[]
[null,"Payment   ",null,null,0]
[]
[30,"Clause 31.0 - Interim payment Clause 31.6.5 shall be deemed to be deletedMaterials and goods stored off site shall not be included in the amount authorised for paymentF:................... V:.................. T:.................. ",null,"Item",0]
[]
[31,"Clause 32.0 - Adjustment to the contract value Notwithstanding the provision of clause 32.13 or any other clause, all fluctuations in costs, with the exception of fluctuations in the rate of Value Added Tax, shall be for the account of the contractor F:..................... V:....................... T:................... ",null,"Item",0]
[]
[32,"Clause 33.0 - Recovery of expense and loss F:...................... V:....................... T:..................... ",null,"Item",0]
[]
[33,"Clause 34.0 - Final account and final payment  F:.................... V:................... T:................... ",null,"Item",0]
[]
[34,"Clause 35.0 - Payment to other parties  F:...................... V:.................... T:................... ",null,"Item",0]
[]
[null,"Termination ",null,null,0]
[]
[35,"Clause 36.0 - Termination by employer - contractor's default F:.................... V:.................... T:...................... ",null,"Item",0]
[]
[36,"Clause 37.0 - Termination by employer - loss and damage F:.................. V:.................. T:................... ",null,"Item",0]
[]
[37,"Clause 38.0 - Termination by contractor - employer's default F:.................. V:................... T:.................... ",null,"Item",0]
[]
[38,"Clause 39.0 - Termination - cessation of the works F:..................... V:................... T:................... ",null,"Item",0]
[]
[null,"Dispute   ",null,null,0]
[]
[39,"Clause 40.0 - Settlement of disputes  F:...................... V:................. T:................. ",null,"Item",0]
[]
[null,"Contract agreement ",null,null,0]
[]
[40,"Clause 41.0 - Post tender provisions  ",null,"Item",0]
[]
[41,"Clause 42.0 - Contractual agreement ",null,"Item",0]
[]
[null,"CONTRACT DATA EMPLOYER - CONTRACTOR The JBCC series 2000 Principal Building Agreement Edition 5.0 Contract Data - Employer to Contractor addendum contains all variables referred to in the Principal Building Agreement that are the responsibility of the Employer to provide the appropriate information that is necessary for the to complete his tender.",null,null,0]
[]
[null,"2.0 CONTRACT AND SITE INFORMATION2.1 Law applicable to this agreement:",null,null,0]
[]
[42,"3.0 INSURANCES AND SECURITIES  As per Contract Data section ",null,"Item",0]
[]
[43,"4.0 PRACTICAL COMPLETION DATES AND PENALTIES  As per Contract Data section ",null,"Item",0]
[]
[44,"5.0 DOCUMENTS AND GENERAL  As per Contract Data Section and Bills of Quantities ",null,"Item",0]
[]
[45,"6.0 CHANGES MADE TO THE STANDARD JBCC DOCUMENT  As per the Contract Data section ",null,"Item",0]
[]
[null,"SECTION B -  PRELIMINARIES  ",null,"H1",0]
[]
[null,"Definitions and interpretation  ",null,null,0]
[]
[46,"Clause 1.0 - Definitions and interpretation F:................... V:.................... T:.................... ",null,"Item",0]
[]
[null,"Documents   ",null,null,0]
[]
[47,"Clause 2.1 - Checking of documents F:.................. V:..................... T:........................ ",null,"Item",0]
[]
[48,"Clause 2.2 - Provisional bills of quantities These bills of quantities are provisionally measured and the subsequent trades are budgetary allowances F:..................... V:.................... T:....................... ",null,"Item",0]
[]
[49,"Clause 2.3 - Availability of construction documentation - Yes  F:..................... V:..................... T:...................... ",null,"Item",0]
[]
[50,"Previous work and adjoining properties ",null,"Item",0]
[]
[51,"Clause 3.1 - Previous work - dimensional accuracy F:................... V:.................... T:...................... ",null,"Item",0]
[]
[52,"Clause 3.2 - Previous work - defects F:.................... V:.................... T:....................... ",null,"Item",0]
[]
[53,"Clause 3.3 - Inspection of adjoining properties  F:....................... V:...................... T:............... ",null,"Item",0]
[]
[54,"Interests of agents (B2.4)  F:....................... V:...................... T:............... ",null,"Item",0]
[]
[55,"Priced documents (B2.5)  F:....................... V:...................... T:............... ",null,"Item",0]
[]
[56,"Tender submission (B2.6)  F:....................... V:...................... T:............... ",null,"Item",0]
[]
[57,"Management of contract (B4)  ",null,"Item",0]
[]
[58,"Management of the works (B4.1)  F:....................... V:...................... T:.............. ",null,"Item",0]
[]
[59,"Programme for the works (B4.2)  F:....................... V:...................... T:............ ",null,"Item",0]
[]
[60,"Progress meetings (B4.3)  F:....................... V:...................... T:............... ",null,"Item",0]
[]
[61,"Technical meetings (B4.4)  F:....................... V:...................... T:............... ",null,"Item",0]
[]
[62,"Labour and Plant records (B4.5)  F:....................... V:...................... T:............. ",null,"Item",0]
[]
[null,"Samples, shop drawings and manufacturer's instructions ",null,null,0]
[]
[63,"Clause 4.1 - Samples of materials F:..................... V:...................... T:.............. ",null,"Item",0]
[]
[64,"Clause 4.2 - Workmanship samples F:.................... V:...................... T:................ ",null,"Item",0]
[]
[65,"Clause 4.3 - Shop drawings  F:..................... V:..................... T:............ ",null,"Item",0]
[]
[66,"Clause 4.4 - Compliance with manufacturer's instructions  F:.................... V:.................. T:.................... ",null,"Item",0]
[]
[null,"Deposits and fees ",null,null,0]
[]
[67,"Clause 5.1 - Deposits and fees F:...................... V:................... T:....................... ",null,"Item",0]
[]
[68,"Enclosure of the works (B6.2)  F:................. V:...................... T:............... ",null,"Item",0]
[]
[69,"Advertising (B6.3)  F:....................... V:...................... T:............... ",null,"Item",0]
[]
[70,"Plant, equipment, sheds and offices (B6.4)  F:............ V:................. T:............. ",null,"Item",0]
[]
[71,"Main notice board (B6.5)  F:............. V:...................... T:............... ",null,"Item",0]
[]
[72,"Subcontractors' notice board (B6.6)  F:....................... V:...................... T:............... ",null,"Item",0]
[]
[null,"Temporary services ",null,null,0]
[]
[73,"Clause 6.1 - Water  F:................... V:..................... T:............ ",null,"Item",0]
[]
[74,"Clause 6.2 - Electricity  F:.................... V:...................... T:............. ",null,"Item",0]
[]
[75,"Clause 6.3 - Telecommunication facilities  F:................... V:.................... T:.............. ",null,"Item",0]
[]
[76,"Clause 6.4 - Ablution facilities  F:.................... V:................... T:.............. ",null,"Item",0]
[]
[null,"Prime cost amounts  ",null,null,0]
[]
[77,"Clause 7.1 - Responsibility for prime cost amounts  F:.................... V:..................... T:.................... ",null,"Item",0]
[]
[null,"Attendance on N/S Subcontractors (B9)  ",null,null,0]
[]
[78,"General attendance (B9.1) ",null,"Item",0]
[]
[79,"Special attendance on n/s subcontractors  ",null,"Item",0]
[]
[80,"Clause 8.1 - Special attendance F:.................... V:....................... T:..................... ",null,"Item",0]
[]
[null,"Financial aspects (B10)  ",null,null,0]
[]
[81,"Statutory taxes, duties and levies (B10.1)  F:....................... V:...................... T:............... ",null,"Item",0]
[]
[82,"Payment of preliminaries (B10.2) Option [A] / [B]  shall apply ",null,"Item",0]
[]
[83,"Adjustment of preliminaries (B10.3)  F:....................... V:...................... T:............... ",null,"Item",0]
[]
[84,"Payment certificate cash flow (B10.4)  F:....................... V:...................... T:............... ",null,"Item",0]
[]
[null,"General   ",null,null,0]
[]
[85,"Clause 9.1 - Protection of the works  F:...................... V:.................... T:.............. ",null,"Item",0]
[]
[86,"Clause 9.2 - Protection/isolation of existing/sectionally occupied works F:..................... V:..................... T:............. ",null,"Item",0]
[]
[87,"Clause 9.3 - Security of the works  F:.................... V:..................... T:............. ",null,"Item",0]
[]
[88,"Clause 9.4 - Notice before covering work F:..................... V:...................... T:........................ ",null,"Item",0]
[]
[89,"Clause 9.5 - Disturbance F:...................... V:.................... T:......................... ",null,"Item",0]
[]
[90,"Clause 9.6 - Environmental disturbance F:..................... V:..................... T: ...................... ",null,"Item",0]
[]
[91,"Clause 9.7 - Works cleaning and clearing  F:.................... V:...................... T:........... ",null,"Item",0]
[]
[92,"Clause 9.8 - Vermin  F:.................. V:................... T:....................... ",null,"Item",0]
[]
[93,"Clause 9.9 - Overhand work  F:........................ V:...................... T:........................ ",null,"Item",0]
[]
[94,"Instruction manuals and guarantees (B11.10)  F:....................... V:...................... T:............... ",null,"Item",0]
[]
[95,"As built information (B11.11)  F:....................... V:...................... T:............... ",null,"Item",0]
[]
[96,"Tenant Installations (B11.12)  F:....................... V:...................... T:............... ",null,"Item",0]
[]
[97,"Site instructions  Instructions issued on site are to be recorded in triplicate in a site instruction book which is to be maintained on site by the contractor  F:................... V:....................... T:....................... ",null,"Item",0]
[]
[null,"Schedule of variables  ",null,null,0]
[]
[null,"Information necessary for elections and completion of those clauses contained in the schedule which are necessary for tender purposes is given hereunder.  Where no information is given it shall mean that no specific requirements are expected or that the clause is not relevant to this specific contract  ",null,null,0]
[]
[null,"10.1 - Provisional bills of quantities [clause 2.2] The quantities are provisional No ",null,null,0]
[]
[null,"10.2 - Availability of construction documentation [clause 2.3] Construction documentation is complete Yes ",null,null,0]
[]
[null,"10.3 - Previous work - dimensional accuracy [clause 3.1] ",null,null,0]
[]
[null,"10.4 Interest of agents (B2.4) N/A ",null,null,0]
[]
[null,"10.5 Defined works area (B3.1) As per Scope of Works, etc. ",null,null,0]
[]
[null,"10.6 Geotechnical investigation (B3.2) YES ",null,null,0]
[]
[null,"10.7 Existing premises occupied (B3.4) YES ",null,null,0]
[]
[null,"10.8 Previous work - dimensional accuracy (B3.4)  N/A ",null,null,0]
[]
[null,"10.9 Previous work - defects [clause 3.2]  N/A ",null,null,0]
[]
[null,"10.10 Services - known (B3.7)  YES ",null,null,0]
[]
[null,"10.11 Protection of trees (B3.9) N/A ",null,null,0]
[]
[null,"10.12 Inspection of adjoining properties [clause 3.3] ",null,null,0]
[]
[null,"10.13 Enclosure of the works (B6.2) YES ",null,null,0]
[]
[null,"10.14 Offices (B6.4.3) YES ",null,null,0]
[]
[null,"10.15 Main notice board (B6.5) YES ",null,null,0]
[]
[null,"10.16 Subcontractors notice board (B6.6) A notice board is required No ",null,null,0]
[]
[null,"10.17 - Water [clause 7.2] Option A (by Contractor)    Yes ",null,null,0]
[]
[null,"10.18 - Electricity [clause 7.3] Option A (by Contractor)  Yes ",null,null,0]
[]
[null,"10.19 - Telecommunications [clause 7.4]  Telkom (by Contractor) YES ",null,null,0]
[]
[null,"10.20 - Ablution facilities [clause 7.5] Option A (by Contractor)    YES ",null,null,0]
[]
[null,"10.21 - Protection of the works [clause 9.1] ",null,null,0]
[]
[null,"10.22 - Protection/isolation of existing/sectionally occupied works  [clause 9.2] Protection/isolation is required      ",null,null,0]
[]
[null,"10.23 - Disturbance [clause 9.5] ",null,null,0]
[]
[null,"10.24 - Environmental disturbance [clause 9.6] ",null,null,0]
[]
[null,"Post tender information (B12.2) ",null,null,0]
[]
[null,"10.25 Payment of preliminaries Alternative selected:   ",null,null,0]
[]
[null,"10.26 Adjustment of preliminaries Alternative selected:  ",null,null,0]
[]
[null,"10.27 Additional agreed preliminaries items   ",null,null,0]
[]
[null,"SECTION  C - SPECIFIC PRELIMINARIES ",null,"H1",0]
[]
[98,"Site instructions  Instructions issued on site are to be recorded in triplicate in a site instruction book which is to be maintained on site by the contractor  F:................... V:....................... T:....................... ",null,"Item",0]
[]
[99,"Warranties for material and workmanship  Where warranties for materials and/or workmanship are called for, the contractor shall obtain a written warranty, addressed to the employer, from the firm supplying the materials and/or doing the work and shall deliver same to the principal agent on the certified completion of the contract. The warranty shall state that workmanship, materials and installation are warranted for a specified period from the date of final completion and that any defects that may arise during the specified period shall be made good at the expense of the firm supplying the materials and/or doing the work, upon written notice to do so. The warranty will not be enforced if the work is damaged by defects  in the construction of the building in which case the responsibility for replacement shall rest entirely with the contractor  F:.......................V:.........................T:............................ ",null,"Item",0]
[]
[100,"Co-operation of contractor for cost management  It is specifically agreed that the contractor accepts the obligation of assisting the principal agent in implementing proper cost management. The contractor will be advised by the principal agent of all cost management procedures which will be implemented to ensure that the final building cost does not exceed the budget. The principal agent undertakes to make available to the contractor all budgetary allowances and cost assessments/reports to enable the proper procedure to be implemented and the contractor shall attend all cost plan review and cost management meetings. The contractor undertakes to extend these procedures, as necessary, to all subcontractors  F:...........................V:.........................T:......................... ",null,"Item",0]
[]
[101,"Propping of floors below  The contractor is advised that propping of floors below may be required if he wishes to use any areas of completed suspended reinforced concrete slabs for vehicle access, storage of materials and goods and location of plant, scaffolding, etc.  The location of these areas and any necessary propping shall be approved by the principal agent and the cost thereof shall be borne by the contractor  F:..................... V:...................... T:................... ",null,"Item",0]
[]
[102,"Agreement: Code of conduct for Contractors  The Contractor must comply with the agreement: Code of Conduct for Contractors, as per DBSA requirements  F:.................... V:....................... T:.........................  ",null,"Item",0]
[]
[103,"Rules and Regulations  The Contractor must comply with the Rules and Regulations (as per DBSA requirements)  F:....................... V:.................... T:...................... ",null,"Item",0]
[]
[104,"LOCAL LABOUR It is a general requirement of this contract that persons normally resident in the locality of the works (local labour) be given preference for employment on the contract. Provided, however, that should adequate and appropriate labour not be available within the locality, other may be employed subject to satisfactory proof being provided that every reasonable endeavour has been made to employ local labour. The Contractor shall identify the local community leaders with the purpose of negotiating with them regarding the utilization of local labour in the construction process. In this regard, the Contractor shall furthermore give preference, wherever possible to the employment of single heads of households, women and youth. The Contractor shall, in general, maximize the involvement of the local community.F:........................... V:........................ T:.................... ",null,"Item",0]
[]
[105,"LABOUR RECORD  At the end of each week the contractor shall provide the principal agent with written record, in schedule form, reflecting the number and description of tradesmen and labours employed by him and all subcontractors on each day.  F:.......................... V:......................... T:..................... ",null,"Item",0]
[]
[106,"C13 HIV/AIDS AwarenessIt is required of the contractor to thoroughly study the HIV/AIDS Specification (HIV 1 to HIV 4) of the Department of Public Works, which must be read together with and is deemed to be incorporated under this section of the Bills of Quantities. Provision for pricing of HIV/AIDS awareness is made under C13.1 to C13.5 hereafter and it is explicitly pointed out that all requirements of the aforementioned specification are deemed to be priced hereunder, as the said items represent the only method of measurement and no additional items or extras to the contract in this regard shall be entertainedThe contractor must take note that compliance with the HIV/AIDS Specification is compulsory. In the event of partial or total non-compliance, the F:......................... V:....................... T:.................. ",null,"Item",0]
[]
[107,"C13.1 Awareness Champion  Selection, appointment, briefing and making available of an Awareness Champion including provision of all relevant services, all in accordance with the HIV/AIDS Specification.  F....................... V............................ T...................... ",null,"Item",0]
[]
[108,"C13.3 Posters, Booklets, Videos, etc.Provision, displaying, maintaining and replacing when necessary of four plastic laminated posters, booklets and educational videos, etc. for the F.................. V....................... T.......................... ",null,"Item",0]
[]
[109,"C13.4 Access to condoms  Provision and maintenance of condom dispensers fixed in position, including male and female condoms, replenish male and female condoms on a daily basis as required  for the duration of the construction period, all in accordance with the HIV/AIDS Specification.  F............................ V..................... T......................... ",null,"Item",0]
[]
[110,"C13.5 Monitoring  Monitoring HIV/AIDS awareness of workers, providing the principal agent with access to information including making available all reports, thoroughly completed and reflecting the correct information, for the duration of the construction period, all in accordance with the HIV/AIDS Specification.  F.................. V.................... T.......................... ",null,"Item",0]
[]
[111,"C14 Occupational Health and Safety Act No. 85 of 1993  Bidders are to allow for costs in providing  a \"Construction Phase Safety, Health and Environmental Plan\". Bidders are further reminded that it is their responsibility to amend their safety plan if the assessed risk of the work changes in the slightest manner.  F................. V....................... T................. ",null,"Item",0]
[]
[null,"COMMUNITY LIAISON OFFICER (CLO) ",null,"H1",0]
[]
[112,"It is a requirement of this Contract that a Community Liaison officer (CLO) be appointed for the area represented by the Tender. The function of the CLO shall be to represent the local community in matters concerning the use of local labour on the works and to assist with and facilitate communication between the Contractor, the Principal Agent and the local communities. The period of appointment of the CLO shall be as stated in the Contract for Temporary Employment as a Community Liaison officer referred to below. It must be noted that the date of commencement of temporary employment of the CLO shall be no later than the date of commencement of the Contract. The identification of the approved CLO to be appointed by the Contractor under the Contract shall be resolved by the Contractor, the particular Ward Councillors in collaboration with the Local Communities and reported to Principal Agent.It will be required, therefore, that the successful Tenderer (i.e. the Contractor) enter into a contract for the employment of the above-mentioned CLO. The contract will be between the Contractor and the CLO, all costs involved shall be borne by the Contractor and the tender shall be deemed to include for this. ",null,"Item",0]
[]
[113,"Contractor to pay the Community Liaison Officer a minimum R10 000.00 per month for the 6 month contract period. ",null,"Item",6,{"v":10000,"d":"10,000.00"}]
[]
[null,"SUMMARY OF CATEGORIES ",null,null,0]
[]
[null,"Category : Fixed  R.........................................................                                  Category:  Value  R.........................................................                                     Category: Time     R....................................................... ",null,null,0]
[]
[{"$nulls":4},0]
[]
[null,"BILL NO. 1 ",null,"H1",0]
[]
[null,"ALTERATIONS",null,"H1",0]
[]
[null,"The tenderer is referred to the \"Model Preambles for Trades 2008\" for supplementary and comprehensive expansion of descriptions, appropriate provision for which shall be deemed to have been included in all relevant rates ",null,"H3",0]
[]
[null,"SUPPLEMENTARY PREAMBLES ",null,"H2",0]
[]
[null,"View site",null,"H4",0]
[]
[null,"Before submitting his tender the tenderer shall visit the site and satisfy himself as to the nature and extent of the work to be done and the value of the materials salvageable from the alterations.  No claim for any variations of the contract sum in respect of the nature and extent of the work or of inferior or damaged materials will be entertained",null,null,0]
[]
[null,"Explosives",null,"H4",0]
[]
[null,"No explosives whatsoever may be used for alteration purposes unless otherwise stated",null,null,0]
[]
[null,"General",null,"H4",0]
[]
[null,"The contractor shall carry out the whole of the works with as little mess and noise as possible and with a minimum of disturbance to tenants in the building and to adjoining premises and their tenants.  He shall provide proper protection and provide, erect and remove when directed, any temporary tarpaulins that may be necessary during the progress of the works, all to the satisfaction of the principal agent",null,null,0]
[]
[null,"Doors, fanlights, windows, fittings, frames, linings, etc which are to remain the property of the employer shall be carefully taken out, temporarily stored, transported over a distance of approximately 100km to store and handed over to the employer",null,null,0]
[]
[null,"Doors, fanlights, windows, fittings, frames, linings, etc which are to be re-used shall be thoroughly overhauled before refixing including taking off, easing and rehanging, cramping up, re-wedging as required and making good cramps, dowels, etc, and oiling, adjusting and repairing ironmongery as necessary, replacing any glass damaged in removal or subsequently and stopping up all nail and screw holes with tinted plastic wood to match timber, unless otherwise described. Re-painting or re-varnishing is given separately",null,null,0]
[]
[null,"Prices for taking out of doors, windows, etc shall include for removal of all beads, architraves, ironmongery, etc",null,null,0]
[]
[null,"Prices for taking out and removing doors and frames shall include for removing door stops, cabin hooks, etc",null,null,0]
[]
[null,"With regard to building up of openings in existing walls, cement screeds and pavings, granolithic, tops of walls, etc, shall be levelled and prepared for raising of brickwork",null,null,0]
[]
[null,"Making good of finishes shall include making good of the brick and concrete surfaces onto which the new finishes are applied, where necessary",null,null,0]
[]
[null,"The contractor will be required to take all dimensions affecting the existing buildings on the site and he will be held solely responsible for the accuracy of all such dimensions where used in the manufacture of new items (doors, windows, fittings, etc)",null,null,0]
[]
[null,"REMOVAL OF EXISTING WORK",null,"H2",0]
[]
[null,"Breaking up and removing concrete",null,"H4",0]
[]
[1,"Unreinforced concrete slab not exceeding 1500mm wide and not exceeding 200mm thick.",null,"m3",42]
[]
[2,"Reinforced concrete slab not exceeding 1500mm wide and not exceeding 200mm thick",null,"m3",5]
[]
[null,"Breaking down and removing brickwork etc ",null,"H3",0]
[]
[3,"One brick walls in beam filling. ",null,"m2",63]
[]
[null,"Taking out and removing doors, windows, etc, including thresholds, sills, etc and making good cement plaster into reveals, lintel and cill ",null,"H3",0]
[]
[4,"Timber single door and frame 813 x 2032m high overall from one brick wall. ",null,"No",9]
[]
[null,"Taking down and removing roofs,etc ",null,"H3",0]
[]
[5,"Take down and remove existing asbestos roof coverings including timber purlins, trusses, etc. complete by registered service provider for the removal and disposal of Asbestos",null,"m2",631]
[]
[6,"Take down and remove existing asbestos gutters including downpipes, accessories etc. and cart away from site by a registered service provider for the removal and disposal of asbestos. ",null,"m",240]
[]
[7,"Asbestos removal and disposal Certificate",null,"Item",1]
[]
[8,"Take down and remove existing fascia boards complete  ",null,"m",192]
[]
[9,"Take down and remove existing barge boards complete  ",null,"m",136]
[]
[null,"Taking down and removing ceilings, etc ",null,"H3",0]
[]
[10,"Gypsum plasterboard ceilings including cornices, timber brandering, etc ",null,"m2",560]
[]
[null,"Taking out and removing ironmongery ",null,"H3",0]
[]
[11,"Mortice lockset from timber door ",null,"No",9]
[]
[null,"Hacking up/off and removing loose plaster, etc from brickwork and preparing surfaces for new plaster, etc ",null,"H3",0]
[]
[12,"Internal plaster from walls ",null,"m2",918]
[]
[13,"External plaster from walls ",null,"m2",918]
[]
[null,"Taking out/off and removing glass ",null,"H3",0]
[]
[14,"Glass from steel windows, including cleaning out rebates and preparing for new glass ",null,"m2",47]
[]
[null,"Take up and remove wood block floor covering, vinyl floor covering,carpeting, waterproofing, etc.",null,"H3",0]
[]
[15,"Vinyl tile floor covering including preparing screed for new floor covering.",null,"m2",428]
[]
[null,"Hacking up/off and removing granolithic, screeds, plaster, etc from concrete or brickwork and preparing surfaces for new screeds, plaster, etc.",null,"H3",0]
[]
[16,"30mm Screed from floors",null,"m2",428]
[]
[null,"Taking out and removing piping, sanitary fittings, etc including disconnecting piping from fittings and making good floor and wall finishes (making good tiling and paintwork elsewhere)",null,"H3",0]
[]
[17,"110mm PVC piping including fittings and brackets",null,"m",250]
[]
[18,"50mm PVC piping including fittings and brackets",null,"m",250]
[]
[19,"Damaged Vitreous china WC pan and cistern",null,"No",15]
[]
[20,"Damaged Vitreous china WC pan with flush valve",null,"No",15]
[]
[null,"MAKING GOOD OF FINISHES ETC ",null,"H2",0]
[]
[null,"Making good internal cement plaster ",null,"H3",0]
[]
[21,"Walls in patches ",null,"m2",89]
[]
[null,"Making good external cement plaster ",null,"H3",0]
[]
[22,"Walls in patches ",null,"m2",89]
[]
[null,"Making good facebrick  ",null,"H3",0]
[]
[23,"Allow for Jet Cleaning and applying new brick dressing ",null,"m2",63]
[]
[24," Repairs to Masonry cracks",null,"m",54]
[]
[null,"Making good roof tiles",null,"H3",0]
[]
[25,"Removal and Replacement of damaged double roman roof tiles to match existing",null,"m2",115]
[]
[null,"TESTING EXISTING WASTE WATER PIPE SYSTEM",null,"H2",0]
[]
[26,"Allow for Testing existing waste water pipe system",null,"Item",1]
[]
[null,"BUDGETARY ALLOWANCES",null,"H2",0]
[]
[null,"EXISTING IRONMONGERY, ETC   ",null,"H3",0]
[]
[null,"Service, repair and make good existing ironmongery, glass, putty , hinges, frames, etc,",null,"H4",0]
[]
[27,"Budgetary allowance for servicing windows complete and leave in perfect working order",null,"Item",1]
[]
[28,"Profit @ 10%",null,"Item",1]
[]
[29,"Attendance @ 5%",null,"Item",1]
[]
[{"$nulls":4},0]
[]
[null,"BILL NO. 2 ",null,"H1",0]
[]
[null,"MASONRY",null,"H1",0]
[]
[null,"The tenderer is referred to the \"Model Preambles for Trades 2008\" for supplementary and comprehensive expansion of descriptions, appropriate provision for which shall be deemed to have been included in all relevant rates ",null,"H3",0]
[]
[null,"SUPPLEMENTARY PREAMBLES ",null,"H2",0]
[]
[null,"BRICKWORK",null,"H3",0]
[]
[null,"Sizes in descriptions",null,"H4",0]
[]
[null,"Where sizes in descriptions are given in brick units, \"one brick\" shall represent the length and \"half brick\" the width of a brick",null,null,0]
[]
[null,"Bagged and sealed walls",null,"H4",0]
[]
[null,"Walls in two skins described as \"bagged and sealed\" shall be deemed to include having the outer face of the inner skin bagged with 1:6 cement and sand mixture and sealed with two coats bitumen emulsion waterproofing coating.",null,null,0]
[]
[null,"Face bricks ",null,"H4",0]
[]
[null,"Bricks shall be ordered timeously to obtain uniformity in size and colour",null,null,0]
[]
[null,"Pointing ",null,"H4",0]
[]
[null,"Descriptions of recessed pointing to fair face brickwork and face brickwork shall be deemed to include square recessed, hollow recessed, weathered pointing, etc",null,null,0]
[]
[null,"BLOCKWORK",null,"H3",0]
[]
[null,"Concrete masonry units",null,"H4",0]
[]
[null,"Blocks are to be either solid or hollow modular dense concrete masonry units having a compressive strength of 7MPa",null,null,0]
[]
[null,"Wall ties for blockwork",null,"H4",0]
[]
[null,"Wall ties shall be polypropylene ties complying with BS 76377.  Ties for hollow walls shall be of sufficient length to allow not less than 75mm of each end to be built into the blockwork.  Ties are to be spaced at intervals of not more than 1m in the horizontal direction and not more than 400mm staggered in the vertical direction except at openings, vertical joints or ends of walls where they are to be placed vertically above each other",null,null,0]
[]
[null,"Blockwork ",null,"H4",0]
[]
[null,"Blockwork shall comply with SANS 10145 \"Concrete Masonry Construction\" ",null,null,0]
[]
[null,"Surfaces to be plastered shall have joints raked out to a depth of at least 10mm to provide a key.  Cavities of hollow walls shall be kept free of mortar droppings or other undesirable matter. Every second perpend of the bottom course of the external skin of hollow walls shall be left open as a weep hole.",null,null,0]
[]
[null,"Standard complementary blocks",null,"H4",0]
[]
[null,"Descriptions of blockwork shall be deemed to include standard complementary blocks such as corner, three-quarter, half and quarter blocks required in the construction of corners, reveals, jambs, ends, etc to solid and hollow walls and for bonding as necessary",null,null,0]
[]
[null,"DECORATIVE BLOCKS",null,"H3",0]
[]
[null,"Blocks shall be of approved manufacture, sound, well burnt or cured and uniform and true in size, shape and colour",null,null,0]
[]
[null,"Where sizes in descriptions are given in brick units, \"one brick\" shall represent the length and \"half brick\" the width of a brick. ",null,"H2",0]
[]
[null,"BRICKWORK ",null,"H2",0]
[]
[null,"SUPERSTRUCTURE ",null,"H2",0]
[]
[null,"Brickwork of NFP bricks in class II mortar ",null,"H3",0]
[]
[1,"Half brick wall",null,"m2",120]
[]
[2,"One brick walls ",null,"m2",213]
[]
[null,"BRICKWORK SUNDRIES ",null,"H3",0]
[]
[3,"Forming toothings and bonding new brickwork to existing ",null,"m2",25]
[]
[null,"2,5mm Brickwork reinforcement ",null,"H3",0]
[]
[4,"150mm wide reinforcement ",null,"m",186]
[]
[null,"Galvanised hoop iron ties, etc (Provisional)",null,"H3",0]
[]
[5,"32 x 1,6mm Wall tie 300mm long with one end shot pinned to brickwork and other end bent out and built into brickwork ",null,"No",400]
[]
[6,"32 x 1,6mm Wall tie 600mm long with one end shot pinned to brickwork and other end bent out and built into brickwork ",null,"No",400]
[]
[7,"32 x 1.6mm Roof tie 1,5m long with one end built 8 courses into brickwork and other end wrapped around and spiked to timber rafters",null,"No",400]
[]
[null,"Facebrick to brickwork in horizontal stretcher bond pointed with recessed horizontal and vertical joints  ",null,"H3",0]
[]
[8,"Extra over for facebrick to match existing ",null,"m2",127]
[]
[null,"NUTEC FIBRE-CEMENT WINDOW SILLS",null,"H2",0]
[]
[null,"\"Everite\" Dark Fibre Cement Cills Complete with Build-In Brackets",null,"H3",0]
[]
[9,"15mm Thick x 150mm wide cill complete with build-in brackets bedded flat and slightly projecting on a cement and sand (1:3)mortar bed",null,"m",120]
[]
[{"$nulls":4},0]
[]
[null,"BILL NO. 3 ",null,"H1",0]
[]
[null,"ROOF COVERINGS, CLADDINGS, ETC",null,"H1",0]
[]
[null,"The tenderer is referred to the \"Model Preambles for Trades 2008\" for supplementary and comprehensive expansion of descriptions, appropriate provision for which shall be deemed to have been included in all relevant rates ",null,"H3",0]
[]
[null,"PROFILED METAL SHEETING AND ACCESSORIES",null,"H2",0]
[]
[null,"0,80mm Thick \"Safintra\" Aluminium G4 Colortech Widedek profile roof sheeting, fixed to intermediate timber purlins at 1400mm centres and to ridge and eaves purlins at 1050mm centres, with 12 x 55mm long Fixtite® or Safintra approved Hex Head self-drilling screws at every second crest at intermediate purlins and every crest at eaves purlins all in accordance with the manufacturer’s recommendations ",null,"H3",0]
[]
[1,"Roof covering with pitches not exceeding 25 degrees",null,"m2",1198]
[]
[2,"Standard galvanised ridge capping screwed through sheeting to purlin",null,"m",253]
[]
[3,"Sondor IBR pattern polyclosure to undersides on ridge capping",null,"m",253]
[]
[4,"Chromadeck metal closure",null,"m",196]
[]
[null,"ROOF AND WALL INSULATION ",null,"H2",0]
[]
[null,"Sisalation 420 heavy industrial grade aluminium foil based insulation",null,"H3",0]
[]
[5,"Insulation cut to size and laid taut over purlins within the ceiling void, off cuts to be inserted between the ceiling and rafter to ensure complete coverage ",null,"m2",1198]
[]
[{"$nulls":4},0]
[]
[null,"BILL NO. 4 ",null,"H1",0]
[]
[null,"CARPENTRY AND JOINERY",null,"H1",0]
[]
[null,"The tenderer is referred to the \"Model Preambles for Trades 2008\" for supplementary and comprehensive expansion of descriptions, appropriate provision for which shall be deemed to have been included in all relevant rates ",null,"H3",0]
[]
[null,"SUPPLEMENTARY PREAMBLES ",null,"H2",0]
[]
[null,"Fixing",null,"H4",0]
[]
[null,"Items described as \"nailed\" shall be deemed to be fixed with hardened steel nails or pins, or to be shot-pinned, to brickwork or concrete",null,null,0]
[]
[null,"Items described as \"plugged\" shall be deemed to include screwing to fibre, plastic or metal plugs at not exceeding 500mm centres, and where described as \"bolted\", the bolts have been given elsewhere",null,null,0]
[]
[null,"PLATE NAILED TIMBER ROOF TRUSS CONSTRUCTION ETC ",null,"H2",0]
[]
[null,"SUPPLEMENTARY PREAMBLES ",null,"H2",0]
[]
[null,"Dimensions in descriptions of trusses are nominal and actual measurements are to be obtained from the architect/engineer and/or taken on site before design or fabrication commences. ",null,"H3",0]
[]
[1,"Design, supply and install timber Roof truss system complete in accordance with standard building regulations, temporary and permanent bracing etc. (elsewhere measured). ",null,"m2",662]
[]
[null,"SA Pine ",null,"H3",0]
[]
[2,"38 x 76mm Wall plates ",null,"m",112]
[]
[3,"76 x 114mm purlins including additional support for trusses and hurricane clips, etc.",null,"m",842]
[]
[4,"76 x 114mm false timber to be fixed on trusses for barge board purlins",null,"m",56]
[]
[5,"38 x 76mm bracing",null,"m",58]
[]
[null,"EAVES, VERGES, ETC ",null,"H2",0]
[]
[null,"Marley' PVC fascia boards ",null,"H3",0]
[]
[6,"12 x 225mm Fascia boards including H-profile jointing strips ",null,"m",112]
[]
[null,"Marley' PVC socketless barge boards ",null,"H3",0]
[]
[7,"12 x 200 x 800mm high Barge boards including H-profile jointing strips ",null,"m",56]
[]
[null,"DOORS ETC ",null,"H2",0]
[]
[null,"TDM Hardwood BB doors hung to steel frames ",null,"H3",0]
[]
[8,"40mm Framed, ledged and braced batten door 813 x 2032mm high of 40 x 150mm wide double top rail and stiles, 20 x 150mm middle ledge and braces and 20 x 225mm double bottom ledge, filled in with 20mm tongued and grooved V-jointed one side vertical boarding with tongued and grooved joints to top rail and stiles and with inner edges of framing and abutting edges of boarding chamfered to form V-joint ",null,"No",9]
[]
[null,"NOTICEBOARDS, KEYBOARDS, DUCKBOARDS, ETC",null,"H2",0]
[]
[null,"Softboard",null,"H4",0]
[]
[9,"12mm Pinning boards glued to plastered walls",null,"No",28]
[]
[null,"FITTINGS",null,"H2",0]
[]
[null,"CUPBOARDS TO KITCHENS, CLASSROOMS, ETC",null,"H3",0]
[]
[null,"SUPPLEMENTARY PREAMBLES",null,"H4",0]
[]
[null,"General",null,"H4",0]
[]
[null,"The following cupboard fittings are given as complete units i.e. the components of the units have not been given separately. Descriptions of such units shall, therefore, be deemed to include all components, assembling, housing, notching, glueing, blocking, planting-on and screwing with countersunk screws, edge strips, thermosetting plastic laminate, glass, ironmongery, metalwork, paint or varnish finishes, etc  Prices are to include for all necessary filler pieces against walls etc",null,null,0]
[]
[10,"Sink cupboard type 2700mm wide x 600mm deep x 900mm high with sides, bottom, divisions, shelf, back and double hinged doors (sink elsewhere)",null,"No",1]
[]
[{"$nulls":4},0]
[]
[null,"BILL NO. 5",null,"H1",0]
[]
[null,"CEILINGS, PARTITIONS AND ACCESS FLOORING",null,"H1",0]
[]
[null,"The tenderer is referred to the \"Model Preambles for Trades 2008\" for supplementary and comprehensive expansion of descriptions, appropriate provision for which shall be deemed to have been included in all relevant rates ",null,"H3",0]
[]
[null,"Fixing",null,"H4",0]
[]
[null,"Items described as \"nailed\" shall be deemed to be fixed with hardened steel nails or pins, or to be shot-pinned, to brickwork or concrete",null,null,0]
[]
[null,"Items described as \"plugged\" shall be deemed to include screwing to fibre, plastic or metal plugs at not exceeding 500mm centres, and where described as \"bolted\", the bolts have been given elsewhere",null,null,0]
[]
[null,"Ceilings",null,"H4",0]
[]
[null,"Unless otherwise described ceilings shall be deemed to be horizontal",null,null,0]
[]
[null,"NAILED-UP CEILINGS",null,"H3",0]
[]
[null,"6mm \"Everite Nutec\" fibre-cement flush boards with H-type pressed steel jointing strips ",null,"H3",0]
[]
[1,"Ceilings including 38 x 38mm sawn softwood brandering at 450mm centres in both directions. ",null,"m2",2105]
[]
[2,"Extra-over for 600 x 600mm trap door including sawn and wrot framing fitted flush with ceiling ",null,"No",6]
[]
[null,"\"Everite Nutec\" fibre-cement cornices ",null,"H3",0]
[]
[3,"50 x 19mm angle rounded cornice ",null,"m",858]
[]
[null,"INSULATION ",null,"H2",0]
[]
[null,"Non-combustible polyester thermal insulation of a density of not less than 10kg/m3 ",null,"H3",0]
[]
[4,"100mm Insulation in blanket form closely fitted and laid on top of brandering between roof timbers etc ",null,"m2",2105]
[]
[{"$nulls":4},0]
[]
[null,"BILL NO 6",null,"H1",0]
[]
[null,"FLOOR COVERINGS, WALL LININGS, ETC",null,"H1",0]
[]
[null,"The tenderer is referred to the \"Model Preambles for Trades 2008\" for supplementary and comprehensive expansion of descriptions, appropriate provision for which shall be deemed to have been included in all relevant rates ",null,null,0]
[]
[null,"Fixing",null,"H4",0]
[]
[null,"Floor coverings, wall linings, etc shall, where applicable, be fixed with adhesive as recommended by the manufacturers of the flooring, linings, etc",null,null,0]
[]
[null,"FLOOR COVERINGS",null,"H2",0]
[]
[null,"300 x 300 x 2,0mm \"Floorflex\" semi-flexible vinyl tiles or equally approved",null,"H4",0]
[]
[1,"Vinyl coverings: On Floors",null,"m2",2105]
[]
[null,"SKIRTINGS, NOSINGS, ETC",null,"H2",0]
[]
[null,"Wrought meranti:",null,"H3",0]
[]
[2,"100mm high x 16mm Meranti Skirting fixed to walls including 19mm quadrant bead planted on. ",null,"m",858]
[]
[null,"POLISH, SEALERS, ETC",null,"H2",0]
[]
[3," Apply 3 coats of water based floor dressing complying to SABS 1042 on vinyl flooring",null,"m2",2105]
[]
[{"$nulls":4},0]
[]
[null,"BILL NO. 7",null,"H1",0]
[]
[null,"IRONMONGERY",null,"H1",0]
[]
[null,"The tenderer is referred to the \"Model Preambles for Trades 2008\" for supplementary and comprehensive expansion of descriptions, appropriate provision for which shall be deemed to have been included in all relevant rates ",null,"H3",0]
[]
[null,"SUPPLEMENTARY PREAMBLES ",null,"H2",0]
[]
[null,"Proprietary items",null,"H4",0]
[]
[null,"Where applicable the manufacturers' names or product catalogue titles are given in sub-headings preceding the items  Prices are to be based on the specific products/articles specified.  If tenderer's wish to offer alternative products/articles for certain items, these items are to be clearly marked and the alternative specification given with supporting brochures etc clarifying the features of the products/articles offered  On request returnable samples are to be provided to the principal agent for consideration",null,null,0]
[]
[null,"HINGES, BOLTS, ETC",null,"H2",0]
[]
[1,"50 x 25mm LD Polished barrel bolt ",null,"No",17]
[]
[null,"LOCKS",null,"H2",0]
[]
[null,"Union ",null,"H3",0]
[]
[2,"Union profile double cylinder lockset ",null,"No",13]
[]
[3,"MG47  47mm Padlock ",null,"No",9]
[]
[null,"LETTERS, NAMEPLATES, ETC",null,"H2",0]
[]
[null,"Union AL5066E ",null,"H3",0]
[]
[4,"152 x 152 x 2mm Anodised silver engraved sign ",null,"No",10]
[]
[{"$nulls":4},0]
[]
[null,"BILL NO. 8",null,"H1",0]
[]
[null,"METALWORK",null,"H1",0]
[]
[null,"The tenderer is referred to the \"Model Preambles for Trades 2008\" for supplementary and comprehensive expansion of descriptions, appropriate provision for which shall be deemed to have been included in all relevant rates ",null,"H3",0]
[]
[null,"SUPPLEMENTARY PREAMBLES ",null,"H2",0]
[]
[null,"Descriptions of bolts, anchors, etc",null,"H4",0]
[]
[null,"Descriptions of bolts shall be deemed to include nuts and washers",null,null,0]
[]
[null,"Descriptions of expansion anchors and bolts and chemical anchors and bolts shall be deemed to include nuts, washers and mortices in brickwork or concrete",null,null,0]
[]
[null,"Items described as \"holed for bolt(s)\" shall be deemed to exclude the bolts unless otherwise described",null,null,0]
[]
[null,"Items described as \"plugged\" shall be deemed to include screwing to fibre, plastic or metal plugs at not exceeding 600mm centres",null,null,0]
[]
[null,"PRESSED STEEL DOOR FRAMES ",null,"H2",0]
[]
[null,"1.2mm Thick galvanized steel frame with 44mm rebate complete with hoop anchors welded to frame and two pairs 100 x 75mm butt hinges for one brick walls ",null,"H3",0]
[]
[1,"Frame for door 813 x 2 032mm high ",null,"No",12]
[]
[{"$nulls":4},0]
[]
[null,"BILL NO. 9",null,"H1",0]
[]
[null,"PLASTERING",null,"H1",0]
[]
[null,"The tenderer is referred to the \"Model Preambles for Trades 2008\" for supplementary and comprehensive expansion of descriptions, appropriate provision for which shall be deemed to have been included in all relevant rates ",null,"H3",0]
[]
[null,"INTERNAL PLASTER",null,"H2",0]
[]
[null,"SCREEDS",null,"H2",0]
[]
[null,"Screeds wood floated, on concrete",null,"H4",0]
[]
[null,"1:3 Cement plaster screeds wood floated, on concrete",null,"H4",0]
[]
[1,"30mm thick on floors",null,"m2",428]
[]
[null,"Cement plaster steel trowelled, on brickwork",null,"H3",0]
[]
[2,"On walls",null,"m2",63]
[]
[3,"On narrow widths not exceeding 300mm wide",null,"m2",100]
[]
[null,"EXTERNAL PLASTER",null,"H2",0]
[]
[null,"Cement plaster wood floated, on brickwork",null,"H3",0]
[]
[4,"On walls",null,"m2",63]
[]
[5,"On narrow widths not exceeding 300mm wide",null,"m2",100]
[]
[{"$nulls":4},0]
[]
[null,"BILL NO .10",null,"H1",0]
[]
[null,"TILING",null,"H1",0]
[]
[null,"User note",null,"H4",0]
[]
[null,"The tenderer is referred to the \"Model Preambles for Trades 2008\" for supplementary and comprehensive expansion of descriptions, appropriate provision for which shall be deemed to have been included in all relevant rates ",null,null,0]
[]
[null,"Patterns",null,"H4",0]
[]
[null,"Unless otherwise described, tiles shall be laid with continuous joints in both directions",null,null,0]
[]
[null,"Fixing",null,"H4",0]
[]
[null,"Unless described as \"fixed with adhesive to plaster (plaster elsewhere)\" descriptions of tiling on brick or concrete walls, columns, etc shall be deemed to include 1:4 cement plaster backing and descriptions of tiling on concrete floors etc shall be deemed to include 1:3 plaster bedding",null,null,0]
[]
[null,"Tiling described as \"fixed with adhesive on power floated concrete\" shall be deemed to include for approved tiling key-coat",null,null,0]
[]
[null,"Ceramic, porcelain, marble and granite tiles are to be fixed and grouted with suitable adhesives and grouts as recommended by the manufacturer of the tiles",null,null,0]
[]
[null,"WALL TILING",null,"H2",0]
[]
[null,"200 x 200 x 5mm White glazed ceramic tiles on brickwork including cement plaster backing",null,"H4",0]
[]
[1,"On walls in isolated panels, splashbacks, etc not exceeding 1m²",null,"m2",20]
[]
[{"$nulls":4},0]
[]
[null,"BILL NO. 11",null,"H1",0]
[]
[null,"PLUMBING AND DRAINAGE (PROVISIONAL)",null,"H1",0]
[]
[null,"The tenderer is referred to the \"Model Preambles for Trades 2008\" for supplementary and comprehensive expansion of descriptions, appropriate provision for which shall be deemed to have been included in all relevant rates ",null,"H3",0]
[]
[null,"Wire gratings",null,"H4",0]
[]
[null,"Descriptions of gutter outlets etc shall be deemed to include wire balloon gratings",null,null,0]
[]
[null,"Stormwater channels",null,"H4",0]
[]
[null,"Descriptions of channels shall be deemed to include necessary excavation, surface preparation, compaction, etc, and disposal of surplus material on site",null,null,0]
[]
[null,"RAINWATER DISPOSAL",null,"H2",0]
[]
[null," Aluminium gutters and rainwater pipes ",null,"H3",0]
[]
[1,"150 x 150 x 0.6mm thick aluminium seamless gutters including matching rivet mitres internally sealed using silicon mastic",null,"m",590]
[]
[2,"100 x 75 x 0.6mm thick rectangular fluted rainwater downpipes fixed to walls with pre-painted downpipe cleats using nail in anchor fixings at 1000mm centres",null,"m",315]
[]
[3,"Extra over 100mm eaves gutter for outlet including boring 100 x 75mm hole through gutter",null,"No",250]
[]
[4,"Extra over gutter for drop box suitable for 155 x 100mm box gutter",null,"No",30]
[]
[5,"Extra over rainwater pipe for bend ",null,"No",112]
[]
[6,"Extra over 100 x 75mm rainwater pipe for shoe ",null,"m",36]
[]
[7,"Extra over gutter for stopped end",null,"No",36]
[]
[null,"STORMWATER DRAINAGE",null,"H2",0]
[]
[null,"25Mpa/19mm Concrete ",null,"H3",0]
[]
[8,"1000 x 150mm Concrete stormwater channel with 600 x 50mm deep 'V' channel, type 193 fabric reinforcement, on suitable 150mm sub-base material compacted to 93% Mod A.A.S.H.T.O. density, including all necessary excavations, formwork, compaction, grading, carting away, etc ",null,"m",220]
[]
[9,"Extra over for angles, intersections, ends, dressing into sides of catchpits, etc ",null,"No",50]
[]
[null,"REPLACE DAMAGED SANITARY FITTINGS",null,"H2",0]
[]
[null,"STAINLESS STEEL SINK",null,"H3",0]
[]
[10,"Model \"DCBPS 1850\" Double Bowl pot sink with splashback",null,"No",2]
[]
[null,"Water Closets",null,"H3",0]
[]
[11,"VAAL SANITARY WARE Hibiscus Elite vitreous china close coupled suite colour White (Code: 772402) with Hibiscus Jazz thermoset seat (Code: 8531Z0), comprising 90º outlet open rim pan (Code: 772600) with matching 6/3 litre top dual flush cistern (Code: 710740) including lid and fitments.",null,"No",15]
[]
[null,"SANITARY PLUMBING   ",null,"H3",0]
[]
[null,"uPVC pipes  ",null,"H3",0]
[]
[12,"50mm Pipes",null,"m",250]
[]
[13,"110mm Pipes",null,"m",210]
[]
[null,"Extra Over uPVC pipes for fittings",null,"H3",0]
[]
[14,"50mm Access bend",null,"No",53]
[]
[15,"110mm Bend",null,"No",53]
[]
[16,"110mm Reducing junction",null,"No",42]
[]
[17,"110mm Pan connector",null,"No",15]
[]
[18,"110mm Access bend",null,"No",22]
[]
[19,"110mm Air vent cowl",null,"No",15]
[]
[null,"REPLACE DAMAGED TRAPS",null,"H3",0]
[]
[20,"40mm \"P\" or \"S\" trap",null,"No",50]
[]
[null,"REPLACE DAMAGED TAPS, VALVES, ETC.",null,"H3",0]
[]
[21,"Straight bowl type urinal flush pipe and spreader ",null,"No",6]
[]
[null,"Sundries",null,"H3",0]
[]
[22,"Hole for 110mm pipe through brickwork",null,"No",15]
[]
[null,"TESTING",null,"H3",0]
[]
[23,"Testing waste pipe system",null,"Item",1]
[]
[{"$nulls":4},0]
[]
[null,"BILL NO. 12",null,"H1",0]
[]
[null,"GLAZING",null,"H1",0]
[]
[null,"The tenderer is referred to the \"Model Preambles for Trades 2008\" for supplementary and comprehensive expansion of descriptions, appropriate provision for which shall be deemed to have been included in all relevant rates ",null,"H3",0]
[]
[null,"GLAZING TO STEEL WITH PUTTY",null,"H2",0]
[]
[null,"4mm Sandblasted glass ",null,"H3",0]
[]
[1,"Panes exceeding 0,1m² and not exceeding 0,5m²",null,"m2",100]
[]
[{"$nulls":4},0]
[]
[null,"BILL NO. 13",null,"H1",0]
[]
[null,"PAINTWORK",null,"H1",0]
[]
[null,"The tenderer is referred to the \"Model Preambles for Trades 2008\" for supplementary and comprehensive expansion of descriptions, appropriate provision for which shall be deemed to have been included in all relevant rates ",null,"H3",0]
[]
[null,"SUPPLEMENTARY PREAMBLES",null,"H2",0]
[]
[null,"PREPARATORY WORK TO EXISTING WORK",null,"H3",0]
[]
[null,"Previously painted plastered surfaces",null,"H4",0]
[]
[null,"Surfaces shall be thoroughly washed down and allowed to dry completely before any paint is applied. Blistered or peeling paint shall be completely removed and cracks shall be opened, filled with a suitable filler and finished smooth",null,null,0]
[]
[null,"Previously painted metal surfaces ",null,"H4",0]
[]
[null,"Surfaces shall be thoroughly rubbed and cleaned down.  Blistered or peeling paint shall be completely removed down to bare metal",null,null,0]
[]
[null,"Previously painted wood surfaces",null,"H4",0]
[]
[null,"Surfaces shall be thoroughly cleaned down.  Blistered or peeling paint shall be completely removed and cracks and crevices shall be primed, filled with suitable filler and finished smooth",null,null,0]
[]
[null,"ON INTERNAL FLOATED PLASTER SURFACES",null,"H2",0]
[]
[null,"One coat alkali resistant primer and two coats PVA emulsion paint for interior use",null,"H4",0]
[]
[1,"Walls",null,"m2",544]
[]
[null,"ON EXTERNAL FLOATED PLASTER SURFACES",null,"H2",0]
[]
[null,"One coat alkali resistant primer and two coats superior quality acrylic emulsion paint for interior and exterior use",null,"H4",0]
[]
[2,"Walls",null,"m2",63]
[]
[null,"ON WOOD SURFACES",null,"H2",0]
[]
[null,"One coat alkyd based universal undercoat and one coat superior quality universal enamel paint",null,"H4",0]
[]
[null,"Spot priming bare wood surfaces, one coat alkyd based universal undercoat and two coats superior quality universal enamel paint",null,"H4",0]
[]
[3,"Roof timbers at eaves and verges",null,"m2",67]
[]
[4,"Barge boards and Facia boards",null,"m2",51]
[]
[null,"Three coats superior quality clear matt varnish",null,"H4",0]
[]
[5,"Doors",null,"m2",100]
[]
[null,"PAINTWORK, ETC TO PREVIOUSLY PAINTED WORK",null,"H2",0]
[]
[null,"ON INTERNAL FLOATED PLASTER SURFACES",null,"H2",0]
[]
[null,"Two coats alkyd based universal undercoat and one coat superior quality universal enamel paint",null,"H4",0]
[]
[6,"Walls",null,"m2",1560]
[]
[null,"ON EXTERNAL FLOATED PLASTER SURFACES",null,"H2",0]
[]
[null,"Two coats superior quality acrylic emulsion paint for exterior use",null,"H4",0]
[]
[7,"Walls",null,"m2",473]
[]
[null,"ON METAL SURFACES",null,"H2",0]
[]
[null,"One coat alkyd based zinc phosphate primer, one coat alkyd based universal undercoat and two coats superior quality universal enamel paint, on steel",null,"H4",0]
[]
[8,"Windows with burglar bars",null,"m2",250]
[]
[9,"Door frames",null,"m2",60]
[]
[{"$nulls":4},0]
[]
[null,"BILL NO. 14",null,"H1",0]
[]
[null,"PROVISIONAL SUMS",null,"H1",0]
[]
[null,"The tenderer is referred to the \"Model Preambles for Trades 2008\" for supplementary and comprehensive expansion of descriptions, appropriate provision for which shall be deemed to have been included in all relevant rates ",null,null,0]
[]
[null,"General",null,"H4",0]
[]
[null,"Work for which budgetary allowances are provided will be measured and valued in accordance with the relevant JBCC Series 2000 Principal Building Agreement (March 2005 Edition) and deducted in whole or in part if not required without any compensation for loss of profit on the said allowances",null,null,0]
[]
[null,"Prime cost amounts and provisional sums are net.  Prime cost amounts shall include for delivery to site of all articles concerned  Provisional sums are for material and equipment supplied and installed complete by firms of specialists",null,null,0]
[]
[null,"Profit",null,"H4",0]
[]
[null,"Where stated, the contractor may allow for profit if required",null,null,0]
[]
[null,"Refer hereunder to \"nominated subcontractors\" or \"selected subcontractors\" or both as the case may be and in accordance with the relevant building agreement (building contract)  Where \"attendance\" is defined in the relevant subcontract agreement/subcontract, the user is to refer thereto and is to ensure that the designations therein are used. Where \"attendance\" is not defined in the relevant subcontract agreement/subcontract, the user is to provide a detailed description of the \"attendance\" required from the contractor",null,null,0]
[]
[null,"General attendance on nominated/selected subcontractors",null,"H4",0]
[]
[null,"Use the following descriptions where the JBCC N/S Subcontract Agreement is applicable",null,null,0]
[]
[null,"The item \"attendance\" which follows each provisional sum for nominated/selected subcontractors' work, shall be deemed to cover all the contractor's costs incurred in providing free of charge to the nominated/selected subcontractors the contractor's duties as described in clause 12.2 of the JBCC N/S Subcontract Agreement",null,null,0]
[]
[null,"Special attendance on nominated/selected subcontractors",null,"H4",0]
[]
[null,"Where \"special attendance\" such as unloading, storing, placing in position, providing special power supplies, specific hoisting, cranage and scaffolding requirements, provision of temporary casing and/or other specific protection of the works, special security and clearing away rubbish is required, a separate item describing the specific requirements in detail is to be provided for the pricing of such requirements",null,null,0]
[]
[null,"Builder's work",null,"H4",0]
[]
[null,"Builder's work in connection with specialist services is given elsewhere in these bills of quantities",null,null,0]
[]
[null,"BUDGETARY ALLOWANCES",null,"H2",0]
[]
[1,"Provide the sum of R400 000.00 for Parkhomes",null,"Item",1,{"v":400000,"d":"400,000.00"},{"v":400000,"d":"400,000.00"}]
[]
[2,"Allow for profit ",null,"%"]
[]
[3,"Allow for attendance ",null,"%"]
[]
[null,"ELECTRICAL INSTALLATIONS (PROVISIONAL)",null,"H3",0]
[]
[null,"General electrical installation",null,"H4",0]
[]
[4,"Provide the sum of R 1 000 000.00 for general electrical installation",null,"Item",1,{"v":1000000,"d":"1,000,000.00"},{"v":1000000,"d":"1,000,000.00"}]
[]
[5,"Allow for profit ",null,"%"]
[]
[6,"Allow for attendance ",null,"%"]
[]
[null,"MECHANICAL INSTALLATIONS (PROVISIONAL)",null,"H3",0]
[]
[null,"General electrical installation",null,"H4",0]
[]
[7,"Provide the sum of R  300 000.00 for general mechanical installation",null,"Item",1,{"v":300000,"d":"300,000.00"},{"v":300000,"d":"300,000.00"}]
[]
[8,"Allow for profit ",null,"%"]
[]
[9,"Allow for attendance ",null,"%"]
[]
[null,"LABORATORY WORKSTATIONS (PROVISIONAL)",null,"H3",0]
[]
[10,"Provide the sum of R 300 000.00 for built-in Laboratory Workstations etc",null,"Item",1,{"v":300000,"d":"300,000.00"},{"v":300000,"d":"300,000.00"}]
[]
[11,"Allow for Profit ",null,"%"]
[]
[12,"Allow for Attendance ",null,"%"]
[]
[null,"APPOINTMENT OF CLO",null,"H3",0]
[]
[10,"Make alllowance of R100 000.00 for appointment of CLO for the project duration of 10 months",null,"Item",1,{"v":100000,"d":"100,000.00"},{"v":100000,"d":"100,000.00"}]
[]
[]
[]
[null,"CPD BUILD PROGRAMME"]
[]
[null,"Note to tenderers: As CPGs may not provide any bidder a competitive advantage. Provisional amounts and fixed percentages for profit and attendance have been provided. Only the provisional amount will be adjusted once the awarded tender amount and/or the beneficiaries have been appointed, and the final values have been ascertained. "]
[]
[null,"MINIMUM TARGETED LOCAL BUILDING MATERIAL MANUFACTURERS"]
[null,"Provision is made for the Minimum Targeted Local Building Material Manufacturers CPG in the execution of this project as described in   C3.1 Project Specifications.  Allowance for monitoring and monthly reporting on material purchased from Local Building Material Manufacturers by main contractor and subcontractors based on determination by Employer taking into account specific project variables","PS",1,{"v":17356.417500000003,"d":"17356.42"}]
[null,"Allowance for profit and attendance, all inclusive of associated costs to the contractor for implementation. ","%"]
[]
[null,"Allowance for attendance all inclusive of associated costs to the contractor for implementation. ","%"]
[]
[null,"MINIMUM TARGETED LOCAL BUILDING MATERIAL SUPPLIERS "]
[null,"Provision is made for the Minimum Targeted Local Building Material Suppliers CPG in the execution of this project as described in   C3.1 Project Specifications. Allowance for monitoring and monthly reporting on material purchased from Local Building Material Suppliers by main contractor and subcontractors based on determination by Employer  taking into account specific project variables ","PS",1,{"v":17356.417500000003,"d":"17356.42"}]
[null,"Allowance for profit all inclusive of associated costs to the contractor for implementation. ","%"]
[null,"Allowance for attendance all inclusive of associated costs to the contractor for implementation. ","%"]
[]
[null,"MINIMUM TARGETED ENTERPRISE DEVELOPMENT"]
[null,"A provisional amount has been allowed for in the execution of this project as described in  C3.1 Project Specifications. The provisional amount allowed is for the appointment of training coordinator, mentor, training service providers and training of the beneficiary enterprises including monitoring and monthly reporting.","PS",1,{"v":173564.17500000002,"d":"173564.18"}]
[null,"Allowance for profit all inclusive of associated costs to the contractor for implementation. ","%"]
[null,"Allowance for attendance all inclusive of associated costs to the contractor for implementation. ","%"]
[]
[null,"LABOUR INTENSIVE PARTICIPATION GOAL"]
[null,"Labour Intensive Participation Goal - Allowance for monthly reporting of labour intensive works by main contractor based on determination by Employer taking into account specific project variables. Allowance for monitoring and monthly reporting on Works executed by means of Labour Intensive methods by main contractor and subcontractors based on determination by Employer taking into account specific project variables ",null,1,{"v":72000,"d":"72000.00"}]
[null,"Allowance for profit all inclusive of associated costs to the contractor for implementation. ","%"]
[null,"Allowance for attendance all inclusive of associated costs to the contractor for implementation. ","%"]
[]
[]
[1,"ALTERATIONS",null,"Page",31]
[]
[2,"MASONRY",null,"Page",35]
[]
[3,"ROOF COVERINGS",null,"Page",36]
[]
[4,"CARPENTRY AND JOINARY",null,"Page",39]
[]
[5,"CEILINGS, PARTITIONS AND ACCESS FLOORING",null,"Page",41]
[]
[6,"FLOOR COVERINGS, WALL LININGS,ETC",null,"Page",42]
[]
[7,"IRONMONGERY",null,"Page",44]
[]
[8,"METALWORK",null,"Page",45]
[]
[9,"PLASTERING",null,"Page",46]
[]
[10,"TILING",null,"Page",47]
[]
[11,"PLUMBING AND DRAINAGE",null,"Page",50]
[]
[12,"GLAZING",null,"Page",51]
[]
[13,"PAINTWORK",null,"Page",54]
[]
[14,"PROVISIONAL SUMS",null,"Page",57]
[]
[null,"BILL NO. 1",null,"H1",0]
[]
[null,"GENERAL SITEWORKS",null,"H1",0]
[]
[null,"The tenderer is referred to the \"Model Preambles for Trades 2008\" for supplementary and comprehensive expansion of descriptions, appropriate provision for which shall be deemed to have been included in all relevant rates ",null,"H3",0]
[]
[null,"GENERAL",null,"H3",0]
[]
[1,"Allow for watering the works by spraying to prevent any nuisance from dust, etc., and supply, erect and remove at completion all temporary dust screens, etc., required",null,"Item",1]
[]
[2,"Allow for protecting all existing work liable to suffer damage from damage during the building operations, alterations, etc., and make good all work damaged with new material to match existing to the approval of the Principal Agent.",null,"Item",1]
[]
[null,"TEMPORARY BARRIERS, SCREENS, ETC.",null,"H3",0]
[]
[null,"Temporary barriers, screens, etc.",null,"H4",0]
[]
[3,"1800mm High IBR sheeting fixed to timber or gum pole posts, bearers, etc.",null,"m",100]
[]
[4,"Extra over for single gate 1000 x 2100mm high, including steel frame, padlock, etc.",null,"No",1]
[]
[5,"Extra over for double gate 6000 x 2100mm high, including steel frame, padlock, etc.",null,"No",1]
[]
[6,"Allow for directional safety, regulatory signage, etc. to barriers, screens, etc.",null,"Item",1]
[]
[7,"Allowance for removal of hoarding, gate, etc. and making good areas disturbed.",null,"Item",1]
[]
[null,"SITE CLEARENCE",null,"H3",0]
[]
[8,"Digging up and removing rubbish, debris, vegetation, hedges, shrubs, bush, etc. and trees not exceeding 200mm girth.",null,"m2",156]
[]
[9,"Stripping average 150mm thick layer of top soil an depositing material in prescribed stock piles on site.",null,"m2",156]
[]
[{"$nulls":4},0]
[]
[null,"BILL NO. 2",null,"H1",0]
[]
[null,"CONCRETE STORMWATER CHANNELS ETC",null,"H1",0]
[]
[null,"The tenderer is referred to the \"Model Preambles for Trades 2008\" for supplementary and comprehensive expansion of descriptions, appropriate provision for which shall be deemed to have been included in all relevant rates ",null,"H3",0]
[]
[null,"EARTHWORKS (PROVISIONAL)",null,"H1",0]
[]
[1,"Excavation in earth not exceeding 2m deep for trenches",null,"m3",378]
[]
[2,"Risk of collapse of sides of excavations not exceeding 1,5m deep",null,"m2",660]
[]
[null,"REINFORCED CONCRETE CAST ON/IN FORMWORK",null,"H2",0]
[]
[3,"25MPa/19mm reinforced concrete in bottoms and sides",null,"m3",30]
[]
[null,"CONCRETE SUNDRIES",null,"H2",0]
[]
[4,"Finishing concrete bottoms smooth with a steel trowel to falls",null,"m2",156]
[]
[null,"TEST CUBES",null,"H2",0]
[]
[5,"Making and testing 150 x 150 x 150mm concrete strength test cube (Provisional)",null,"No",8]
[]
[null,"Formwork",null,"H4",0]
[]
[6,"Rough formwork to sides",null,"m2",120]
[]
[7,"Smooth formwork to sides above sloping bottoms",null,"m2",120]
[]
[8,"10mm Expansion joints with soft-board through concrete bottoms not exceeding 300mm high",null,"m",110]
[]
[null,"REINFORCEMENT (PROVISIONAL)",null,"H2",0]
[]
[null,"Fabric reinforcement",null,"H4",0]
[]
[9,"Type 193 fabric reinforcement in concrete bottoms and sides",null,"m2",156]
[]
[null,"STORMWATER DRAINAGE",null,"H2",0]
[]
[null,"Class 100D concrete pipes:",null,"H3",0]
[]
[10,"450mm Pipes laid in and including trenches exceeding 1m and not exceeding 2m deep.",null,"m",135]
[]
[null,"Sumps, catchpits, inspection chambers, etc.",null,"H3",0]
[]
[11,"Grid inlet chamber size 760 x 450mm not exceeding 1m deep internally to invert level formed of hard burnt one brick sides in 1:3 cement mortar on and including 200 mm thick mass concrete (class 25 /19 concrete at 28 days) bottom projecting 50 mm beyond sides and mass concrete (class 25/19 concrete at 28 days) benching, rendered internally in 1:3 cement plaster with 100 x 100 x 8mm Galvanised angle iron support to top cover and 150 mm thick Precast Concrete cover slab reinforced with Y10 bars at 100c/d kerb on top, rebated for and fitted with cast iron double seal cover and frame (cover and frame elsewhere) in accordance with SABS 558, bedded in 1:3 cement mortar and sealed in tallow, including all necessary channels and fittings, excavations, formwork, holes through sides for pipes.",null,"No",5]
[]
[{"$nulls":4},0]
[]
[null,"BILL NO. 3",null,"H1",0]
[]
[null,"WATER SUPPLIES",null,"H2",0]
[]
[null,"The tenderer is referred to the \"Model Preambles for Trades 2008\" for supplementary and comprehensive expansion of descriptions, appropriate provision for which shall be deemed to have been included in all relevant rates ",null,null,0]
[]
[null,"Plastic water tanks etc:",null,"H3",0]
[]
[1,"5000 Litre roto molded or equal approved plastic tank complete with lid, side inlet and outlet, and 4 No. galvanised 4mm stay wires 2.5m each long connected to tank, and including fixing to steel platform.",null,"No",12]
[]
[null,"WATER TANK SUPPORTS (ALL TRADES) (PROVISIONAL)",null,"H2",0]
[]
[2,"Provide new concrete tank base including all necessary earthworks, brickwork, concrete, formwork and reinforcement with 5000 litre water tank overall size; 2250 x 1800mm High including bibtap in accordance with Engineers drawings",null,"No",12]
[]
[{"$nulls":4},0]
[]
[null,"BILL NO. 4",null,"H1",0]
[]
[null,"WALKWAYS, RAMPS,STEPS,ETC",null,"H2",0]
[]
[null,"The tenderer is referred to the \"Model Preambles for Trades 2008\" for supplementary and comprehensive expansion of descriptions, appropriate provision for which shall be deemed to have been included in all relevant rates",null,null,0]
[]
[null,"THE FOLLOWING IN UNCOVERED WALKWAYS, RAMPS, STAIRS, ETC",null,"H3",0]
[]
[null,"Coarse river sand filling supplied by the contractor:",null,"H3",0]
[]
[1,"Under floors etc.",null,"m3",45]
[]
[null,"Approved brand of anti-termite soil poison applied by a Registered Pest Control Company and guaranteed against termite infestation for ten years:",null,"H3",0]
[]
[2,"Treat filling under concrete floor with 'Chlordane Heptachlor Aldrin' or equal approved.",null,"m2",150]
[]
[null,"Reinforced 25Mpa/19mm Concrete:",null,"H3",0]
[]
[3,"Surface beds cast in panels on waterproofing.",null,"m3",15]
[]
[4,"Ramps.",null,"m3",5]
[]
[null,"Finishing top surfaces of concrete smooth with a wood float:",null,"H3",0]
[]
[5,"Surface beds, slabs, etc to falls and currents.",null,"m2",150]
[]
[null,"Smooth Formwork (Degree of Accuracy II)",null,"H3",0]
[]
[6,"Edges, risers, ends and reveals not exceeding 300mm high.",null,"m",160]
[]
[null,"Test blocks",null,"H3",0]
[]
[7,"Making and testing set of three 150x150x150mm concrete strength test cubes.",null,"No",9]
[]
[null,"Expansion joints with bitumen impregnated softboard between vertical concrete or brick surfaces:",null,"H3",0]
[]
[8,"10mm Joints not exceeding 300mm high.",null,"m",50]
[]
[null,"Fabric reinforcement:",null,"H3",0]
[]
[9,"Type 193 fabric reinforcement in concrete surface beds, slabs, etc.",null,"m2",150]
[]
[null,"Waterproofing under Surface beds",null,"H3",0]
[]
[10,"350 Micron USB orange polyethylene dampproof membrane in accordance with SABS 952 Type C laid on sand bed (elsewhere measured).",null,"m2",150]
[]
[{"$nulls":4},0]
[]
[1,"GENERAL SITEWORKS",null,"Page",60]
[]
[2,"STORMWATER DRAINAGE",null,"Page",62]
[]
[3,"WATER SUPLLIES",null,"Page",63]
[]
[4,"WALKWAYS ,RAMPS, STEPS ETC",null,"Page",65]
[]
[null,"SUMMARY PAGE"]
[1,"PRELIMINARIES",null,"Page",25]
[]
[2,"BUILDING WORKS",null,"Page",58]
[]
[3,"EXTERNAL WORKS (PROVISIONAL)",null,"Page",66]
[]
[null,"Sub Total",null,"ST",0]
[]
[null,"ADD 5% of contingencies"]
[]
[null,"Sub Total",null,"ST",0]
[]
[null,"ADD: Value Added Tax @ 15%",null,"TAX",{"v":0.15,"d":"15%"}]
[]
[null,"Sub Total",null,"ST",0]