{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Mnaual Valves"],"not_rendered":{"images":1,"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"Mnaual Valves","index":0,"n_rows":18,"n_cols":16,"rows_kept":18,"merged":[[0,1,0,4],[0,5,0,9],[0,10,0,14],[1,1,1,3],[2,0,3,0],[2,1,3,1],[2,2,3,2],[2,3,3,3],[2,4,2,5],[2,6,2,7],[2,8,3,8],[2,9,3,9],[2,10,3,10],[2,11,3,11],[2,12,3,12],[2,13,3,13],[2,14,3,14],[2,15,3,15],[17,1,17,8],[17,12,17,14],[20,1,20,8]]}
[{"$nulls":5}," PTFE Filter Destruction Plant System Valve List\nFor procurement.",{"$nulls":4},"Page 1 of 4"]
[null,"Manual Valves"]
[null,"Valve type ","Valve code","Valve size","Design Conditions",null,"Operating Conditions",null,"Safety Class ","Valve Description","Quantity","NOTES   ","Supplier of Purchase","Lead-time","UNIT PRICING","PRICING"]
[{"$nulls":4},"Temp [°C]","Press.[kPa(g)]","Temp [°C]","Press.[kPa(g)]"]
[1,"Ball Valve ","SB","25 mm",93,20685,35,"-5 to 600","SC  3","Connection ends: RF, B16.5 or NPT-M/F as B1.20.1, Class 1500\nBody: 316 SS, ASTM A182-F316/A351-CF8M\nTrim: 316 SS\nPacking/Seal: Graphite\nBall material: 316 SS\nBonnet/Cap: 316 SS",1]
[2,"Ball Valve ","SB","50 mm",93,1585,"Amb",520,"SC  3","Connection ends: RF, B16.5, Class 150\nBody: 316 SS\nTrim: 316 SS\nPacking/Seal: Graphite\nBall material: 316 SS\nBonnet/Cap: 316 SS",1]
[3,"Ball Valve ","SB","50 mm",375,740,800,-5,"SC  3","Connection ends: RF, B16.5, Class 150\nBody: 316 SS, ASTM A182-F316/A351-CF8M\nTrim: 316 SS\nPacking/Seal: Graphite\nBall material: 316 SS\nBonnet/Cap: 316 SS",1]
[4,"Ball Valve ","SB","100 mm",93,1585,"Amb","-5 to -12","SC  3","Connection ends: RF, B16.5, Class 150\nBody: 316 SS, ASTM A182-F316/A351-CF8M\nTrim: 316 SS\nPacking/Seal: Graphite\nBall material: 316 SS\nBonnet/Cap: 316 SS",6]
[6,"Globe Valve ","SG","15 mm",93,1585,45,600,"SC  3","Connection ends: RF, B16.5 or  NPT-M/F as B1.20.1, Class 150\nBody: 316 SS, ASTM A351 - CF8M\nTrim: 316 SS\nPacking/Seal: API 600\nBall material: 316 SS\nBonnet/Cap: 316 SS",10]
[7,"Globe Valve ","SG","25 mm",93,1585,45,600,"SC  3","Connection ends: RF, B16.5 or  NPT-M/F as B1.20.1, Class 150\nBody: SS 316, ASTM A351 - CF8M\nTrim: 316 SS\nPacking/Seal: API 600\nBall material: 316 SS\nBonnet/Cap: 316 SS",5]
[8,"Globe Valve ","SG","40  mm",93,1585,45,520,"SC  3","Connection ends: RF, B16.5, Class 150\nBody: SS 316, ASTM A351 - CF8M\nTrim: 316 SS\nPacking/Seal: API 600\nBall material: 316 SS\nBonnet/Cap: 316 SS",2]
[9,"Globe Valve ","SG","50 mm",93,1585,45,520,"SC  3","Connection ends: RF, B16.5, Class 150\nBody: 316 SS , ASTM A351 - CF8M\nTrim: 316 SS\nPacking/Seal: API 600\nBall material: 316 SS\nBonnet/Cap: 316 SS",2]
[11,"Non-return Valve","SU","40 mm",93,1585,45,158,"SC  3","Connection ends: RF, B16.5, Class 150\nBody: 316 SS, ASTM A182-F316/A351-CF8M\nTrim: 316 SS\nPacking/Seal: API 600\nBall material: 316 SS\nBonnet/Cap: 316 SS",1]
[12,"Non-return Valve","SU","50 mm",93,1585,30,520,"SC  3","Connection ends: RF, B16.5, Class 150\nBody: 316 SS, ASTM A182-F316/A351-CF8M\nTrim: 316 SS\nPacking/Seal: API 600\nBonnet/Cap: 316 SS",2]
[13," Strainer","SQ","25 mm",93,1585,45,9.1,"SC  3","Connection ends: RF, B16.5 or NPT-F/M B1.20.1, Class 150\nBody: 304/316 SS , ASTM A182-F316/A351-CF8M\nTrim: SS 304/316\nPacking/Seal: GRAPHITE ( supplier to advise) \nBall material: 316 SS\nBonnet/Cap: 316 SS",1]
[14," Strainer","SQ","40 mm",93,1585,45,30.1,"SC  3","Connection ends: RF, B16.15, Class 150\nBody: 304/316 SS, ASTM A182-F316/A351-CF8M\nTrim: 304/316 SS\nPacking/Seal: CAF ( supplier to advise) \nBall material: 316 SS\nBonnet/Cap: 316 SS",1]
[15," Strainer","SQ","50 mm",93,1585,30,"20.8","SC  3","Connection ends: RF, B16.15, Class 150\nBody: 304/316 SS, ASTM A182-F316/A351-CF8M\nTrim: 304/316 SS \nPacking/Seal: CAF ( supplier to advise) \nBall material: 316 SS\nBonnet/Cap: 316 SS",2]
[{"$nulls":9},"Total:",{"$f":"SUM(K5:K17)","v":35},null,"TOTAL:",null,null,{"$f":"SUM( P5:P17)","v":0}]