{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["0163384","Deviation Schedule_0163384","Test Schedule_0163384"],"read":"whole","date_system":"1900"}

{"sheet":"0163384","index":0,"n_rows":54,"n_cols":7,"rows_kept":54,"merged":[[1,1,1,6],[2,1,2,6],[3,1,3,6],[4,1,4,6],[7,2,7,3],[8,2,8,3],[9,3,9,4],[20,3,20,4],[24,3,24,4],[27,2,27,4],[28,2,28,4],[29,3,29,4],[34,3,34,4],[39,3,39,4],[42,1,42,3],[43,1,43,6],[46,1,46,6],[49,1,49,3],[49,5,49,6],[53,1,53,3],[53,5,53,6]]}
[{"$nulls":3},"ESKOM TENDER E2719DXLIMOU"]
[null,"Technical Schedules A and B for"]
[null,"STAYROD 133kN 2400x24 ADJUST Eskom D-DT 7023"]
[null,"Schedule A:  Purchasers specific requirements"]
[null,"Schedule B:  Guarantees and technical particulars of equipment offered"]
[]
[null,1,null,2,null,3,4]
[null,"Item ","Description",null,null,"Schedule A","Schedule B"]
[null,1,"Product Information"]
[null,1.1,"·","Purchasing details"]
[null,"1.1.1",null,"Eskom SAP No",null,{"v":163384,"d":"0163384"},"xxxxxxxxxx"]
[null,"1.1.2",null,"Manufacturer's Name","Manufacturer Name","xxxxxxxxxx"]
[null,"1.1.3",null,"Manufacturer's Product Code","Specify Code","xxxxxxxxxx"]
[null,"1.1.4",null,"Manufacturer's Drawing number & Revision number","Specify No and Rev","xxxxxxxxxx"]
[null,"1.1.5",null,"Manufacturer's unique identifier on product body as per Eskom D-DT 7023","Specify Markings","YES"]
[null,"1.1.6",null,"Manufacturer's strength rating mark on product body as per Eskom D-DT 7023","Specify Markings","YES"]
[null,"1.1.7",null,"Compliance to all dimensions on Eskom Buyer's Guide Drawings","Eskom D-DT 7023 and D-DT 3172","YES"]
[null,"1.1.8",null,"Item sample required","OEM Only","YES","xxxxxxxxxx"]
[null,"1.1.9",null,"Stayrod to be supplied as a set with:\nTamper proof locking mechanism,\nand Forged Bow & Rachet Nut. \nStayrod must be compatible with a suitable STAY PLATE (SEE D-DT-3172 FOR DETAILS) ","Eskom D-DT 7023 and D-DT 3172","YES"]
[]
[null,1.2,"·","Mechanical Properties"]
[null,"1.2.1",null,"Mechanical failing load","kN",133]
[null,"1.2.2",null,"Material Grade as per EN10025-2 (European Standard)",null,"S355JR Steel"]
[]
[null,1.3,"·","Galvanising"]
[null,"1.3.1",null,"Average minimum galvanising thickness on product body complies to SANS 121",null,"YES"]
[]
[null,2,"Documentation (to be submitted with tender)"]
[null,null,"Note:  All documentation to be provided in electronic format."]
[null,2.1,"·","General"]
[null,"2.1.1",null,"Manufacturer's outline drawings of item","Sets",1]
[null,"2.1.2",null,"Material grade certification",null,"YES"]
[null,"2.1.3",null,"Visual inspection of welds according to Eskom's 240-75883830","As per Eskom 240-75883830","YES"]
[]
[null,2.2,"·","Test Reports (where applicable)",null,"Required","Report\nNumber"]
[null,"2.2.1",null,"Dimensional and material verification (SANS 61284)","Test report submitted","Report number"]
[null,"2.2.2",null,"Galvanising certificate of product body (SANS 61284 and SANS 121)","Test report submitted","Report number"]
[null,"2.2.3",null,"Visual examination  (SANS 61284)","Test report submitted","Report number"]
[]
[null,2.3,"·","Mechanical Tests",null,"Required","Report\nNumber"]
[null,"2.3.1",null,"Damage and failure load test (SANS 61284)","Test report submitted","Report number"]
[null,"2.3.2",null,"Tensile test (SANS 61284 and Eskom 10TB-034)","Test report submitted","Report number"]
[null,"ESKOM TENDER E2719DXLIMOU"]
[null,"NOTE:  DEVIATION SCHEDULE CONTINUE ON NEXT PAGE.\n             IF NO DEVIATIONS ARE MENTIONED ON THE DEVIATION SCHEDULE IT WILL BE ACCEPTED\n             THAT THE SUPPLIER AND MANUFACTURER FULLY COMPLIES WITH THE REQUIREMENTS OF\n             THE ESKOM SPECIFICATON(S)."]
[]
[]
[null,"SUPPLIER SIGNATURES"]
[]
[null,"         "]
[null,"Name (Print)",{"$nulls":3},"Company Name"]
[]
[]
[]
[null,"Sign",{"$nulls":3},"Date"]

{"sheet":"Deviation Schedule_0163384","index":1,"n_rows":45,"n_cols":6,"rows_kept":45,"merged":[[0,0,0,6],[1,0,1,6],[2,0,2,6],[3,0,3,6],[4,0,4,6],[5,2,5,6],[6,2,6,6],[7,2,7,6],[8,2,8,6],[9,2,9,6],[10,2,10,6],[11,2,11,6],[12,2,12,6],[13,2,13,6],[14,2,14,6],[15,2,15,6],[16,2,16,6],[17,2,17,6],[18,2,18,6],[19,2,19,6],[20,2,20,6],[21,2,21,6],[22,2,22,6],[23,2,23,6],[24,2,24,6],[25,2,25,6],[26,2,26,6],[27,2,27,6],[28,2,28,6],[29,2,29,6],[30,2,30,6],[31,2,31,6],[32,2,32,6],[33,2,33,6],[34,2,34,6],[35,2,35,6],[37,1,37,6],[40,1,40,3],[40,5,40,6],[44,1,44,3],[44,5,44,6]]}
["ESKOM TENDER E2719DXLIMOU"]
["Deviation schedule"]
["STAYROD 133kN 2400x24 ADJUST Eskom D-DT 7023"]
["SAP No. 0163384"]
["Any deviations offered to this specification shall be listed below with reasons for deviation.  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective that that specified by Eskom."]
["Item","Clause","Description of Deviation"]
{"$rows_empty":31}
[null,"SUPPLIER SIGNATURES"]
[]
[null,"         "]
[null,"Name (Print)",{"$nulls":3},"Company Name"]
[]
[]
[]
[null,"Sign",{"$nulls":3},"Date"]

{"sheet":"Test Schedule_0163384","index":2,"n_rows":21,"n_cols":6,"rows_kept":21,"merged":[[0,1,0,4],[1,1,1,4],[2,1,2,4],[11,1,11,2],[13,1,13,6],[16,1,16,3],[16,5,16,6],[20,1,20,3],[20,5,20,6]]}
[null,"Test Report Schedule"]
[null,"STAYROD 133kN 2400x24 ADJUST Eskom D-DT 7023"]
[null,"SAP No. 0163384"]
[]
[null,1,2,3,4]
[null,"Item ","Description","Specification","Report No."]
[null,"2.2.1","Dimensional and material verification","SANS 61284"]
[null,"2.2.2","Galvanising certificate of product body","SANS 61284, SANS 121"]
[null,"2.2.3","Visual examination  ","SANS 61284"]
[null,"2.3.1","Damage and failure load test","SANS 61284"]
[null,"2.3.2","Tensile test ","SANS 61284, Eskom 10TB-034"]
[]
[null,null,"ESKOM TENDER E2719DXLIMOU"]
[null,"SUPPLIER SIGNATURES"]
[]
[null,"         "]
[null,"Name (Print)",{"$nulls":3},"Company Name"]
[]
[]
[]
[null,"Sign",{"$nulls":3},"Date"]