{"text_format":"3","workbook":"xls","n_sheets":8,"sheets":["TSHIAWELO","LENZ","MIDWAY","KLIPTOWN","NANCEFIELD ","ORLANDO","MLAMLANKUNZI","NEW CANADA"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"TSHIAWELO","index":0,"n_rows":1271,"n_cols":8,"rows_kept":1271,"merged":[[0,0,0,1],[5,0,5,1],[30,4,30,6],[140,3,140,5],[169,3,169,5],[194,3,194,5],[222,3,222,5],[349,4,349,6],[393,4,393,6],[454,4,454,6],[659,4,659,6],[700,4,700,6],[736,4,736,6],[808,4,808,6],[830,4,830,6],[866,4,866,6],[878,4,878,6],[921,1,921,5],[923,1,923,5],[925,1,925,5],[961,4,961,6],[1189,4,1189,6],[1217,4,1217,6],[1240,1,1240,5],[1242,1,1242,5],[1244,1,1244,5],[1266,1,1266,5],[1268,1,1268,5],[1270,1,1270,5]],"flags":["formulas_cached_only"]}
[]
[]
[null,"SCHEDULE OF QUANTITIES "]
[]
[null,"STATION REFURBISHMENT AT TSHIAWELO STATION: RFQ NO:13/07/2022/08CRES"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
["No"]
[null,"SECTION 1"]
[]
[null,"BILL NO. 1"]
[]
[null,"PRELIMINARY AND GENERAL "]
[]
[null,"Preliminary and General"]
[]
[1,"All Preliminary and General applicable to this project",null,"Sum",1]
[]
[null,"Occupational Health and safety"]
[]
[null,"The contractor shall comply with all the requirements set out in the Construction Regulations, issued under The Occupational Health & Safety Act no 85 of 1993."]
[]
[null,"Safety file shall be provided by the contractor prior to commencement of work."]
[]
[null,"The contractor shall carry out the works with as little noise and mess as possible. All rubble shall be taken away from site on a daily basis."]
[]
[null,"Note: All designated items should comply with local content threshold. "]
[]
[2,"Compliance with Occupational Health and Safety Act (Act 85 of 1993) and its regulations and with the Employers Health and Safety",null,"Sum",1]
[]
[{"$nulls":4},"Carried to final summary"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
["No."]
[null,"SECTION NO. 2"]
[]
[null,"CIVIL AND GENERAL BUILDING WORK AT MIDWAY STATION"]
[]
[null,"BILL NO. 1 "]
[]
[null,"ALTERATIONS  "]
[]
[null,"SUPPLEMENTARY PREAMBLES  "]
[]
[null,"General "]
[]
[null,"Special care shall be exercised during the progress of the"]
[null," work to ensure that any electrical installations, water supply"]
[null," pipes, telephone and other services which may be"]
[null," encountered are not interfered with and notice shall be given"]
[null," to the project manager if any disconnection or"]
[null," alterations become necessary"]
[]
[null,"The contractor shall take all precautions necessary to"]
[null," prevent any nuisance from dust whilst carrying out the work"]
[]
[null,"Leave in good condition"]
[]
[null,"The contractor must leave the existing building,in which "]
[null,"the alterations are executed ,clean and neat at completion"]
[]
[null,"Price shall include removal and disposal of rubble from site"]
[]
[null,"REMOVAL OF EXISTING WORK  "]
[]
[]
[null,"Taking down and removing ceiling"]
[]
[1,"Suspended ceiling",null,"m²",50]
[]
[2,"Rhino Board ",null,"m²",150]
[]
[null,"Taking down and removing doors"]
[]
[3,"Timber single door 813 x 2032",null,"No.",10]
[]
[null,"Taking out and removing glass, beads, etc"]
[]
[4,"Brocken window pane from steel frame including upgrading, cleaning and preparation to receive new",null,"m²",15]
[]
[null,"Hacking up/off and removing ceramic tile floor and wall finishes including removing mortar bed or backing and preparing concrete or brick surface for new screed, plaster or tile finishes"]
[]
[5,"150 x 150mm tiles to walls",null,"m²",50]
[]
[6,"300 x 300mm tiles to floors",null,"m²",50]
[]
[null,"Taking out and removing piping, sanitary fittings, etc including disconnection piping from fittings"]
[]
[7,"9l Ceramic pan and cistern ",null,"m²",15]
[]
[8,"wash hand basin including all fittings",null,"No",7]
[]
[9,"Down pipes",null,"m",50]
[]
[10,"Gutters",null,"m",100]
[]
[null,"Taking out and removing"]
[]
[11,"2000 x 2000mm high blinds",null,"No",15]
[]
[null,"SERVICING, REPAIRING, RE-FIXING, CLEANING, ETC OF EXISTING WORK",null,"No",4]
[]
[null,"Clean down existing roof sheeting, box gutters, flashings. Etc apply de-rusting compound to surfaces, prepare area for paint application and allow for re-fixing, replacing and waterproofing of necessary roof screws, fixing screws, etc"]
[]
[12,"IBR roof sheeting in fair condition not exceeding 30 degree slope",null,"m²",100]
[]
[13,"Sheet steel box gutters in fair condition",null,"m",200]
[]
[null,"Re-fixing and aligning of fascia and barge boards"]
[]
[14,"Fibre cement fascia and barge boards not exceeding 300mm girth",null,"m",50]
[]
[15,"Sheet metal fascia and barge boards not exceeding 300mm girth",null,"m",50]
[]
[null,"Clean down existing facebrick façade, painted walls, plinths, wall tiles, floor tiles, etc with water and brush "]
[]
[16,"Internal and external face brick walls",null,"m²",500]
[]
[17,"Internal ceramic wall and floor tiles",null,"m²",200]
[]
[null,"Clean down existing window panes"]
[]
[18,"Glazing to steel windows measured on both sides",null,"m²",100]
[]
[null,"Clean out and service gutters"]
[]
[19,"125 x 100mm eaves gutter",null,"m",100]
[]
[20,"250 x 200mm industrial eaves gutter",null,"m",100]
[]
[null,"Upgrading of stormwater and Sewer network"]
[]
[21,"High pressure jetting and cleaning of 300mm diameter stormwater underground pipe",null,"m",350]
[]
[22,"High pressure jetting and cleaning of 110mm diameter sewer underground pipe",null,"m",350]
[]
[null,"Servicing existing steel industrial Roll-shutter doors including operating mecanism"]
[]
[24,"3000mm long x 2400mm high steel gate to be delivered at New Canada depot",null,"No.",3]
[]
[{"$nulls":3},"Carried to final summary"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
[]
[null,"BILL NO 2"]
[]
[null,"Earthworks (Provisional)"]
[]
[null,"Supplementary Preambles"]
[]
[null,"All soil poisoning and insecticide to be applied under a ten year guarantee by an approved firm of specialist"]
[]
[null,"General notes"]
[]
[null,"Fill material shall be placed in lift of not more than 150mm"]
[null,"Compaction density to be controlled using DCP apparatus to a maximum of 30mm/blow 93% MOD AASHTO compaction is to be achieved "]
[]
[null,"Where backfill is required on both sides of walls, backfill both sides simultaneously."]
[]
[null,"Where compaction of fill material behind retaining walls is done using mechanical rollers, the rollers must be kept 500mm away from the wall and this 500mm portion must be compacted with hand stampers or wackers."]
[]
[null,"Site Clearance"]
[]
[1,"Cleaning and removal of rubble from site",null,"m²",10000]
[]
[null,"G5 Material  compacted to 93% Mod AASHTO density"]
[]
[2,"Backfilling to trenches",null,"m",300]
[]
[{"$nulls":3},"Carried to final summary"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
[]
[null,"BILL NO 3"]
[]
[null,"CONCRETE WORK"]
[]
[null,"Application: Outdoor Litter Bin"]
[null,"External size: 700mm x 700mm x 875mm high"]
[null,"Internal size: 600mm x 600mm x 700mm deep"]
[null,"Capacity: 320 litres"]
[null,"Mass: 430kg"]
[null,"Finish: Exposed aggregate"]
[null,"Advertising space: 4 x 685mm x 590mm"]
[null,"Drainage hole in bottom"]
[]
[1,"Supply and deliver Advertising Bin with exposed aggregate external finish ",null,"No.",15]
[]
[null,"STEEL BRIDGE TREADS"]
[]
[null,"Reinforced Precast Concrete Bridge Treads"]
[]
[2,"2500mm long x 300mm wide x 80mm deep precast concrete bridge treads as per attached drawing with bending schedule",null,"No.",6]
[]
[{"$nulls":3},"Carried to final summary"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
[]
[null,"BILL NO 4"]
[]
[null,"ROOF COVERING ETC"]
[]
[null,"PROFILE METAL SHEETING AND ACCESSORIES"]
[]
[null,"Roof sheeting to be Concealed Fix interlocking \"KLIP-LOK 700\",  0,58mm thick heavy industrial Z275 spelter galvanised steel sheeting with Chromadek, ColorPlus, Colourbond or Globalcoat finish to one side and Grey other side and accessories, fixed to steel purlins using SL 700  approved clips and fasteners. Cover width 700mm. High wind - 120km/h plus - loading to be considered with installation and fixing must be in accordance with manufacturer's recommendations and specifications."]
[]
[1,"Roof covering with pitch not exceeding 25 degrees",null,"m²",30]
[]
[2,"450mm galvanized steel roll top ridge",null,"m",10]
[]
[null,"REPAIRS TO GALVANISED IRON ROOF COVERING"]
[]
[null,"Carfully examine entire roof area and locate leaks with particular attention"]
[null,"given to roof leaks where marks are available on walls and ceiling.Locate holes"]
[null,"and solder.Replace defective screws using longer screws as ''Reaseal'' or similar"]
[null,"approved as SABS Specification 135 where purlins are fixed on edge,and 6mm "]
[null,"bolts where purlins are fixed on flat.Beat into corrugation damaged or buckled"]
[null,"edges,fix in position where necessary using self tapping screws,roofing screws"]
[null,"or verandah bolts.Similarly examine all flashing,ridging and vally linings,"]
[null,"repair and refix loose sections,as for the roof covering.No plastic or other"]
[3,"compounds are to be used to render leaks watertight.",null,"m²",2000]
[]
[{"$nulls":3},"Carried to final summary"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
[]
[null,"BILL NO. 5"]
[]
[null,"CARPENTRY AND JOINERY  "]
[]
[null,"TIMBER  "]
[]
[null,"All softwood to be South African Pine  "]
[]
[null,"DOORS, ETC"]
[]
[null,"Wrought meranti doors hung to steel frames"]
[]
[null,"44mm thick exterior grade flush solid core timber single door with 3mm thick commercial ply on both sides with consolidated edges fitted and complying with SABS 545 in pressed steel frame. All painted in accordance with architect's colour schedules"]
[]
[1,"813 x 2032 x 44mm single leaf solid core with commercial veneer for paint. pricing shall include painting as per manufactures specification",null,"No.",10]
[]
[2,"1500 x 2032 x 44mm single leaf solid core with commercial veneer for paint. pricing shall include painting as per manufactures specification",null,"No.",1]
[]
[null,"44mm thick interior grade flush solid core timber single door with 3mm thick commercial ply on both sides with consolidated edges fitted and complying with SABS 545 in pressed steel frame. All painted in accordance with architect's colour schedules"]
[]
[3,"813 x 2032 x 44mm single leaf solid core with commercial veneer for paint. pricing shall include painting as per manufactures specification",null,"No.",15]
[]
[null,"FITTINGS"]
[]
[null,"The following in modular timber cupboards, counters, duty stations, desk etc. as per Cupboard Connections Specification"]
[]
[null,"Carcasses of 16mm thick particle board with both faces white melamine with white Masonite backs. Shelving of 16mm particle board, both faces white melamine and front edge in white PVC. Doors of 16mm particle board with post formed vertical edges and laminated in Renolit. Tops of 32mm particle board with post formed leading edges and laminated in high pressure decorative laminate. All butt edges and edges against walls to be sealed with silicon sealant. Hinges to be “Hettich”. Drawer runners to be metal 500mm series with nylon runners or similar. All units complete with door, handles, hinges, cupboards, door, locks, barrel bolts and shelves. Floor unit complete with kick plates. (Formica tops measured elsewhere)   "]
[]
[null,"Built in cupboards fittings"]
[]
[null,"General"]
[]
[null,"The following cupboard fittings have been measured as complete units i.e. the components of the units have not been separately measured. The descriptions, therefore, of such units shall be deemed to include all components, assembling, housing, notching, glueing, blocking, planting on and screwing with countersunk screws, edge strips, decorative plastic finish, glass, ironmongery, metalwork and paint or varnish finishes"]
[]
[null,"Ticket sales work stations"]
[]
[4,"1000H x 700W x 700mmD Floor cupboard with lockable shelf / drawer and single hinged door to match Pollak Park Ticket Office counter (Top measured elsewhere)",null,"No.",4]
[]
[null,"Kitchen cupboards,etc."]
[]
[5,"Kitchen sink floor cupboard 2000 x 600 x 900mm high with sides, bottom, back, 3 hinged doors and one drawer completely working including handles, etc. top and sink measured else where",null,"No.",2]
[]
[null,"Interior type particle board with Formica veneer "]
[]
[6,"900 x30mm thick granite with all exposed edges large bevel edged, fixed to supports using dabs of 100% black silicone adhesive along all supports with all joints filled with matching polyester resin glue. Granite surface to be sealed using an approved stone sealer, all in accordance with the manufacturer's recommendations.",null,"m",20]
[]
[7,"2mm thick edge strip 32mm wide",null,"m",13]
[]
[8,"Cut 50mm work top to fit end bowl sink, measured else where ",null,"No.",6]
[]
[null,"EAVES, VERGES, ETC"]
[]
[null,"Pressed fibre cement"]
[]
[null,"10 x 225mm Fascia’s including galvanized steel H-Profile jointing strips"]
[]
[null,"10 x 230mm Barge boards including galvanized steel H-profile jointing strips "]
[]
[null,"SUPPLEMENTARY PREAMBLES"]
[]
[null,"Particle board shall comply with the following specification"]
[]
[null,"1)      SABS 1300 Particle board: exterior and flooring type"]
[]
[null,"2)      SABS 1301 Particle board: interior type"]
[]
[null,"Description of hardwood joinery shall be deemed to include pelleting of bolt holes"]
[]
[null,"Joinery "]
[]
[null,"Description of frames shall be deemed to include frames, transoms, mullions, rails, etc"]
[]
[null,"Fixing"]
[]
[null,"Items described as “nailed” shall be deemed to be fixed with hardened steel nails or short pims to brickwork or concrete "]
[]
[null,"Items described as “plugged” shall be deemed to include screwing to fibre, plastic or metal plugs at not exceeding 600mm centres, and where described as “bolted” the bolts have been given elsewhere "]
[]
[null,"Decorative"]
[]
[null,"Decorative laminate finish shall be glued under pressure. Edge strips shall be butt jointed at junctions with adjacent similar finish"]
[]
[null,"ROOFS ETC"]
[]
[null,"Plate nailed timber roof truss construction"]
[]
[null,"The following is applicable in respect of roof trusses:"]
[]
[null,"Trusses are at maximum 1000mm centres and with a pitch of "]
[]
[null,"The roof to have 600mm overhang on both sides (along lengths), eaves cladded with 4mm fibre cement ceiling "]
[]
[null,"Roof to have vertical cladded gable end projecting  150mm at ends of the building."]
[]
[null,"The first set of dimensions given with the descriptions are the external dimensions of the building, the second set of dimensions (in brackets) are the external dimensions of the roofs which include the dimensions of the overhangs along lengths and at ends"]
[]
[null,"All trusses are to be fabricated in a factory by specialist approved by the Architect"]
[]
[null,"All trusses shall be designed by a registered Professional Engineer (in accordance with the draft SABS Code of Practice for the Design of Timber Structures)"]
[]
[null,"The Manufacture of the trusses shall supply a written guarantee that the trusses are design, manufactured and erected to support the roof covering specified. The guarantee shall be valid for a period of 10 (ten) years"]
[]
[null,"Sawn softwood "]
[]
[null,"Roof construction to double pitched roof with two gable ends over rectangular shaped building erected in position complete including all trusses, jack rafters, permanent bracing, gang nail plates ( wall plates and purlins measured elsewhere)"]
[]
[9,"Building size 5000 x 5000mm long overall on plan",null,"No.",1]
[]
[]
[null,"Wrought softwood "]
[]
[10,"50 x 75mm purlins at 900mm center’s to sides of trusses ",null,"m",100]
[]
[11,"38mm x 114mm wall plates ",null,"m",50]
[]
[12,"38mm x 100mm Grade M4 ridge beam",null,"m",50]
[]
[13,"50mm x 75mm purlins",null,"m",100]
[]
[null,"Sundries"]
[]
[14,"Two coats creosote on sawn timbers",null,"m²",130]
[]
[{"$nulls":4},"Carried to final summary"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
[]
[null,"BILL NO 6"]
[]
[null,"CEILING WORK"]
[]
[null,"SUPPLEMENTARY PREAMBLES "]
[]
[null,"Description "]
[]
[null,"Items described as “nailed” shall be deemed to be fixed with hardened steel nails or pins or shot pinned to brickwork or concrete"]
[]
[null,"Items described as “plugged” shall be deemed to include screwing to fibre, plastic or metal plugs at not exceeding 600mm centres, and where described as “bolted”, bolts priced elsewhere"]
[]
[null,"Finishes to suspended ceilings:"]
[]
[null,"All finishes to be applied at the factory during the manufacturing process and to be delivered on site “pre-finished” as described. No applying of finishes on site will be allowed"]
[]
[null,"NAILED UP CEILING"]
[]
[null,"6mm “Everite Nutec” fibre cement boards with H-type pressed steel jointing including painting with one coat of alkali resistance primer , one undercoat and two coat eggshell enamel paint"]
[]
[1,"Ceiling generally 600mm wide including 38 x 38mm sawn softwood brandering at maximum 600mm centres nailed to and including 75 x 50mm sawn softwood bearers at 900mm centres suspended approximately 250mm below timber trusses with 75 x 38mm vertical bearers at 600mm centres nailed to tie beams of trusses",null,"m²",150]
[]
[2,"Extra over ceiling for 800 x 800mm trap door of 38 50mm wrought softwood rebated framing with one 38 x 38mm sawn softwood cross brander covered with ceiling board and fitted flush in opening",null,"No.",3]
[]
[null,"“Rhino” gypsum plasterboard cornice"]
[]
[3,"75mm coved cornices fixed to ceiling",null,"m",200]
[]
[null,"SUSPENDED CEILING"]
[]
[null,"OWAcoustic(R) Futura Premium biologically absorbable mineral wool ceiling tiles, NRC - 0.75, size 1200 x 600 x 15mm with Square-edge and white painted finish, laid on fire rated OWAconstruct(R) system S3 exposed demountable  T24 suspension system, comprising galvanised main tees and cross tees with main tees suspended by means of galvanised hangers at centres not exceeding 1200mm with ceiling perimeter finished with OWAconstruct Shadowline W-trim, plugged and screwed at 200mm centres, and all installed to manufacturer's instructions."]
[]
[4,"Suspended ceiling not exceeding 1m below concrete soffit",null,"m²",30]
[]
[null,"Cornices to suspended ceiling"]
[]
[5,"Standard brilliant white pre-painted metal angle cornices plugged",null,"m",50]
[]
[null," Perforated lay-in powder coated aluminium ceiling tiles"]
[]
[{"$nulls":4},"Carried to final summary"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
[]
[null,"BILL NO 7"]
[]
[null,"IRONMONGERY"]
[]
[null,"LOCKS"]
[]
[null,"Supply and install"]
[]
[1,"Ultra-security heavy duty double pin locks",null,"No",10]
[]
[2,"3 liver mortice lockset with handles",null,"No",30]
[]
[3,"Indicator door lock chrome plated",null,"No",15]
[]
[4,"90mm square Padlock",null,"No",10]
[]
[null,"BATHROOM FITTINGS  "]
[]
[5,"Satin stainless-steel toilet roll holders for 2 rolls with central shaft system and cylinder lock, plugged and screwed to the wall with stainless steel screws. (vandal resistant)",null,"No",4]
[null," "]
[null,"Door closer"]
[]
[6,"Heavy duty slide arm door closer",null,"No",5]
[]
[null,"SIGNAGE"]
[]
[null,"External signage"]
[]
[null,"Male Signage"]
[]
[7,"500 x 500 x 3mm mild steel ACM panel with vinyl graphic overlay",null,"No",1]
[]
[null,"Female Signage"]
[]
[8,"500 x 500 x 3mm mild steel ACM panel with vinyl graphic overlay",null,"No",1]
[]
[null,"Paraplegic Signage"]
[]
[9,"500 x 500 x 3mm mild steel ACM panel with vinyl graphic overlay",null,"No",1]
[]
[null,"Double Sided Platform Station Name "]
[]
[10,"2100mm x 3000 x 3mm mild steel ACM panel sprayed to Pantone 3005C with vinyl graphic overlay and white vinyl graphics mounted on 65mm diameter x 2.6m high above the ground mild steel poles in concrete footing ",null,"No",6]
[]
[null,"Stainless Steel Grade 304 Platform Public Seating"]
[]
[null,"Arms and Legs: Aluminium Die-Cat, chromed. "]
[]
[null,"Cross beam: 2mm Aluminium extrusion, silver. "]
[]
[null,"Seat and back: Stainless steel "]
[]
[11,"5 Seater 2890mmW x 670mmD x 785mmH Peforated Aluminium chairs suitable for outdoors burried on earth less then 1mm deep including excavation, concrete, backfilling, etc",null,"No",10]
[]
[null,"ALUMINIUM WINDOWS "]
[]
[12,"Window type HS1812 Bronze Powder coated 1800 x 1200mm high aluminum sliding window",null,"No",1]
[{"$nulls":4},"Carried to final summary"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
[]
[null,"BILL NO 8"]
[]
[null,"PLUMBING WORK "]
[]
[null,"SANITARY FITTINGS"]
[]
[1,"Vandal resistance low level High traffic suite complete (Front flush), suite to includes CC  white Cistern made from high strength technoplast polymer with concealed mounting bracket, heavy duty securing bolts, concealed tamper proof lid screws and hiflo MK3 flush valve, including CC Pan and and heavy duty seat.",null,"No",5]
[]
[2,"Concealed Anti-vandal high traffic suite (Front flush), CC Cistern excluding CC Pan",null,"No",5]
[]
[3,"Paraplegic vitreous china floor mounted paraplegic washdown suite colour White (Code: 7300SC) comprising semi close couple 90º outlet open rim washdown pan and matching 9 litre cistern, including lid, fitments and purpose-made chromium plated side flush lever.\n",null,"No",1]
[]
[4,"Close coupled suite colour White , comprising 90º outlet open rim pan with matching 9 litre front single flush cistern including lid and fitments and Jazz Thermoset seat.",null,"No",7]
[]
[5,"Ceramic wash hand basin colour White, size 510 x 405mm with one tap hole including integrated overflow and chain stay hole bolted to wall with two x 10mm bolts and including Classic floor mounted pedestal and sealed with silicone sealant where basin meets wall.",null,"No",10]
[]
[6,"China drop-in vanity basin colour White (Code: 7034), size 420 x 420mm fitted into opening in granite vanity top (elsewhere specified) and sealed with silicone sealant where basin rim meets vanity top.  To be used in conjunction with wall mounted push on demand tap as specified V05-V06.",null,"No",6]
[]
[null,"URINAL BASIN"]
[]
[7,"Sanitary ware white vitreous wall mounted urinal with top inlet or back inlet . Overall size 600x385x380mm. Supplied with 38mm c.p. domical grating, a spreader(with a 20mm tread) and two hanger brackets",null,"No",3]
[]
[8,"1830 x 1220mm high floor mounted curved manual flush urinal Centre outlet manufactured from stainless steel AISI 304 including 20Mpa/20mm for installation and unreinforced concrete slab",null,"No",1]
[]
[null,"SINK, BASIN, ETC"]
[]
[9,"Grade 430 stainless steel double bowl sink and drainer size 1160 x 460mm with tiling key, 40mm chromium plated flanged outlets and waste unions, vulcanite or rubber plugs, chromium plated chains and stays, 40mm rubber resealing P-trap with extension piece and clamped connections",null,"No.",2]
[]
[null,"TAPS, VALVES, ETC"]
[]
[null,"Supply and install"]
[]
[10,"Self-closing push button tap",null,"No.",10]
[]
[11,"15mm chrome plated deck mounted sink mixer with overarm swivel outlet and adjustable flanges, manufactured in accordance with SANS 226:2004 Type 1.",null,"No.",2]
[]
[12,"Medical elbow action pillar tap with raised nose or equal approved, chrome finish. SANS 226 TYPE 2. ",null,"No.",1]
[]
[13,"15mm brass garden  tap ",null,"No.",2]
[]
[14,"Exposed type urinal flush valve with ball-o-stop, wall flange, chrome plate finish and non-hold open feature",null,"No.",3]
[]
[15,"15mm Ø BSP built-in sleeve, DZR brass urinal flush valve with internal flow control, strainer and no-hold feature for single bowl urinal.",null,"No.",1]
[]
[16,"Flexi connector",null,"No",30]
[]
[17,"15 Brass Gate Valve ",null,"No",4]
[]
[18,"Mini Ball Valve ",null,"No",30]
[]
[19,"22mm Brass Gate Valve including cast iron valve box",null,"No",2]
[]
[null,"WASTE UNINON ETC"]
[]
[20,"Basin waste, plug, chain, stay and backnut  ",null,"No.",10]
[]
[null,"TRAPS ETC"]
[]
[21,"38mm sink “P” trap",null,"No.",10]
[]
[22,"365/40 CP bottle trap 40 x 40 INC CP/PVC adaptor to 40mm suitable for wash hand basin and urinal ceramic basin",null,"No.",5]
[]
[23,"110mm pan connector completely ",null,"No.",14]
[]
[null,"WATER SUPPLIERS"]
[]
[null,"Class “O” copper pipe "]
[]
[24,"15mm pipes ",null,"m",20]
[]
[25,"15mm pipes chased into brick walls and make good",null,"m",35]
[]
[26,"22mm pipes ",null,"m",10]
[]
[27,"22mm pipes chased into brick walls",null,"m",10]
[]
[28,"Extra over class “O” copper pipes for capillary fittings"]
[]
[29,"15mm fitting  ",null,"No.",10]
[]
[30,"22mm fitting  ",null,"No.",5]
[]
[31,"15mm Tee",null,"No.",10]
[]
[32,"22mm Tee",null,"No.",5]
[]
[null,"Galvanized pipe "]
[]
[33,"32mm pipes ",null,"m",10]
[]
[null,"Extra over class Galvanized pipes for capillary fittings"]
[]
[34,"32mm fitting  ",null,"No.",3]
[]
[35,"32mm elbow  ",null,"No.",2]
[]
[36,"32mm Tee",null,"No.",2]
[]
[null,"Plastic pipe"]
[]
[37,"75mm high pressure plastic pipes in trenches less than 2m deep",null,"m",50]
[]
[38,"75mm gate valve",null,"No.",1]
[]
[39,"Male adaptor",null,"No.",6]
[]
[40,"Straight coupling",null,"No.",6]
[]
[null,"Plastic waste pipes"]
[]
[41,"50mm waste pipes with all connection and make good",null,"m",50]
[]
[null,"SOIL DRAINAGE"]
[]
[null,"Upvc class 34 pipes including excavation, bedding, backfilling and compaction and disposal of surplus material"]
[]
[42,"110mm pipes laid in and including trenches not exceeding 1m deep",null,"m",50]
[]
[43,"Extra over Upvc class 34 pipes for fittings",null,"No.",6]
[]
[44,"110 Bend",null,"No.",5]
[]
[45,"110mm junction",null,"No.",4]
[]
[46,"110mm Access bend",null,"No.",2]
[]
[null,"Sundries"]
[]
[47,"110mm Upvc cleaning eye to end of 110 Upvc pipe",null,"No.",2]
[]
[48,"350 x 350 x 50mm thick precast concrete inspection eye marker slab finished smooth on exposed surfaces with letters “I.E” or “I.O” on top and placed flush in ground or paving",null,"No.",2]
[]
[49,"Testing soil drainage system ",null,"Item",1]
[]
[null,"WATER RETICULATION"]
[]
[null,"PREAMBLES"]
[]
[null,"The contractor is referred to the General Preambles for trades 2017 published by the Association of South Africa Quantity Surveyors before pricing"]
[]
[null,"WATER PIPEWORK"]
[]
[null,"HDPE PE 100PN 12.5 pipes including excavation, bedding, backfilling, and compaction and disposal of surplus material"]
[]
[null,"High density polyethylene class 16 pipes"]
[]
[50,"25mm pipes with all other required connections laid in and including trenches ",null,"m",100]
[]
[51,"25mm fitting  ",null,"No.",3]
[]
[52,"25mm elbow  ",null,"No.",2]
[]
[53,"25mm Tee",null,"No.",2]
[]
[54,"Testing water supply system ",null,"Item",1]
[]
[null,"PLATFORM MANHOLE COVERS AND FRAMES"]
[]
[]
[55,"Type 9B MD polymer lid and frame including to make good after completion",null,"No.",5]
[]
[56,"600 x 900mm polymer lid and frame including to make good after completion",null,"No.",10]
[]
[null,"ELECTRIC WATER HEATERS"]
[]
[null,"Supply, deliver and install Electrical geysers with all other accessories  "]
[]
[null,"Hydro boiler"]
[]
[57,"5 litre Stainless steel water boiler , with stainless steel tank, steam free boiling water, electronic controls, 15mm overflow, connected to 15mm cold water supply including isolating valve and 230 volt 1800 watt electrical power supply, plugged and screwed to wall and fitted under 1 year warranty.",null,"No.",2]
[]
[null,"RAIN WATER GOODS"]
[]
[null,"0.8mm galvanized sheet iron"]
[]
[58,"125 x 100mm eaves gutter",null,"m",100]
[]
[59,"Extra over 125 x 100mm eaves gutter for stopped end",null,"No.",20]
[]
[60,"Extra over 125 x 100 eaves gutter for angle",null,"No.",25]
[]
[61,"Extra over 125 x 100mm eaves gutter for outlet for 100 x 75mm pipe",null,"No.",20]
[]
[62,"100 x 75mm rainwater pipes",null,"m",70]
[]
[63,"Extra over 100 x 75mm rainwater pipe for shoe",null,"No.",20]
[]
[null,"0.9mm galvanized sheet iron"]
[]
[64,"250 x 200mm industrial eaves gutter including heavy duty brackets fixed at 500mm centers",null,"m",100]
[]
[65,"Extra over 250 x 200mm eaves gutter for stopped end",null,"No.",10]
[]
[66,"Extra over 250 x 200 eaves gutter for angle",null,"No.",5]
[]
[67,"Extra over 125 x 100mm eaves gutter ",null,"No.",10]
[]
[68,"300mm rainwater pipes",null,"m",50]
[]
[70,"Extra over rainwater pipe for shoe",null,"No.",10]
[]
[{"$nulls":4},"Carried to final summary"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
["No."]
[]
[null,"BILL NO.9"]
[]
[null,"METAL WORK"]
[]
[null,"SECURITY GATES "]
[]
[null,"Supply and install Burglar door"]
[]
[1,"900 x 2100mm high Heavy duty Burglar door and frame with 16mm steel round bar and 40 x 40 x 2.5mm square tubing ",null,"No.",5]
[]
[2,"1500 x 2100mm high Heavy duty Burglar door and frame with 16mm steel round bar and 40 x 40 x 2.5mm square tubing ",null,"No.",1]
[]
[null,"Supply and install Burglar windows"]
[]
[3,"508mm W x 629mm H Box windows guard constructed with 5mm of expanded metal and 50 x 50 x 6mm equal angles.",null,"No.",10]
[]
[null,"Gates"]
[]
[null,"Gates welded to steel footbridge"]
[]
[4,"Supply and Install mild steel welded double swing gate 3m high x 4m wide steel swing gate with heavy duty hinges constructed from 76x50x3.5mm frame, diagonal intermediate steel section of 12x12mm at 100mm centers with heavy duty lock and bullet type hinges completely",null,"No.",2]
[]
[null,"Gates bolted to brickwork or concrete walls"]
[]
[5,"Supply and Install mild steel welded 3000mm high x 10000mm long steel sliding gate constructed from 120x60x4.5mm rectangular frame, intermediate steel section of 2 x 120x60x4.5mm and 1 x 120x60x4.5mm horizontal section including anti-lift system, heavy duty wheels and heavy duty lock completely with 16mm round bar diameter rail in trenches covered by 30 Mpa concrete",null,"No.",1]
[]
[null,"Steel flats sheets welded on gates and bugler doors"]
[]
[6,"3mm thick mild stainless steel plate sheets welded on gates and bugler doors on both sides",null,"m²",40]
[]
[null,"STEEL ROLLER SHUTTERS "]
[]
[null,"Roll-Up Perforated galvanised, SABS 1461, & epoxy coated M/S manually hand chain operated push-up roller shutter for maximum opening 3000 x 3000mm high with standard bottom rail, 75 x 0.8mm thick end-locked slats, 120mm extra-wide tamper proof guides, 4.5mm end plates, closed shaft and 2 x slidebolts, extruded with Aluminium Tbar & Astragal rubber weather seal. Including galv. cover box and powder coated components incl. door curtain, end plates, cover box, guides & T-bar. Door fixed to brick, concrete or structural steel jambs and concrete or steel lintel over. Contractor to provide cavity of 160mm x 120mm for recessing guides"]
[]
[7,"Manual hand chain Push-up Roller Shutters, for openings not exceeding 3000mm x 3000mm high.",null,"No.",8]
[]
[{"$nulls":4},"Carried to final summary"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
[]
[null,"BILL NO.10"]
[]
[null,"GLAZING"]
[]
[null,"GLAZING TO STEEL WITH PUTTY"]
[]
[null,"38mm high penetration resistance clear laminated safety glass"]
[]
[1,"250 X 500mm high BRG viewing panel glazed in 38mm thick bullet resistant glass with one-way vision film",null,"No.",4]
[]
[null,"6.5mm high penetration resistance clear laminated safety glass"]
[]
[2,"Panes exceeding 0.1 m2 and not exceeding 0.5m2",null,"m²",4]
[]
[null,"4mm clear float glass"]
[]
[3,"Panes exceeding 0.1 m2 and not exceeding 0.5m2",null,"m²",20]
[]
[null,"4mm clear obscure glass"]
[]
[4,"Panes exceeding 0.1 m2 and not exceeding 0.5 m2",null,"m²",10]
[]
[null,"Mirrors"]
[]
[null,"6mm silver float glass copper backed mirrors with polished edges holed for and fixed with chromium plated dome capped mirror screws with rubber buffers to plugs in brickwork"]
[]
[5,"Mirror 1000 x 1000mm with four screws",null,"No.",5]
[]
[null,"Bullet Resistant Pay / Transaction Windows including sales windows"]
[]
[6,"38mm x 770mm long x 600mm Level G3 bullet resistant glazed & natural anodized aluminum transaction window with 30mm deep stainless steel dish tray and speech transfer posts (interior applications only), overall size to details, glazed in 38mm thick clear glass with 32mm post formed granite counter top.",null,"No.",5]
[]
[{"$nulls":4},"Carried to final summary"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
[]
[null,"BILL NO.11"]
[]
[null,"PAINTWORK"]
[]
[null,"For preambles see “Model Preambles for Trades” 2008 edition published by the Association of South African Quantity Surveyors "]
[]
[null,"SUPPLEMENTARY PREAMBLES"]
[]
[null,"Previously painted plastered surfaces "]
[]
[null,"Surfaces shall be thoroughly washed down and allowed to dry completely before any paint is applied. Blistered or peeling paint shall be completely removed and cracks shall be opened, filled with a suitable filler and finished smooth"]
[]
[null,"Previously painted metal surfaces "]
[]
[null,"Surfaces shall be thoroughly rubbed and cleaned down. Blistered or peeling paint shall be completely removed down to bare metal"]
[]
[null,"Previously painted wood surfaces "]
[]
[null,"Surfaces shall be thoroughly cleaned down. Blistered or peeling paint shall be completely removed and cracks and crevices shall be primed, filled with a suitable filler and finished smooth"]
[]
[null,"PAINTWORK, ETC TO NEW WORK"]
[]
[null,"ON FLOATED PLASTER"]
[]
[null,"One coat professional plaster primer and two coats of white Professional Superior Low Sheen  "]
[]
[1,"On ceiling and cornices ",null,"m²",200]
[]
[null,"ON WOOD"]
[]
[null,"One coat wood primer, one Universal Undercoat  and two coats Prasa Oakley Brown enamel paint"]
[]
[2,"On doors ",null,"m²",150]
[]
[null,"ON METAL"]
[]
[null,"One coat zinc chromate primer, one under coat  and two coats professional white gloss enamel paint"]
[]
[3,"On buglers, gates, door frames, window frames, rainwater goods etc",null,"m²",200]
[]
[null,"One coat professional plaster primer and two coats contractors Brick and Slasto Dressing/Brick seal"]
[]
[4,"On internal and external face brick walls   ",null,"m²",1000]
[]
[null,"PAINTWORK ETC TO PREVIOUSLY PAINTED WORK"]
[]
[null,"ON METAL"]
[]
[null,"Wash with polycell sugar soap and rinse with clean water to remove all traces of soap, remove all loose flaking paint and repair any cracks and defects, spot prime bare and repaired areas with bonding liquid and apply One coat of waterprime, one coat of universal undercoat, two coats of gloss Enamel of PRASA Grey \n"]
[]
[5,"On footbridge and all steel work",null,"m²",3000]
[]
[null,"ON FLOATED PLASTER"]
[]
[null,"Wash with polycell sugar soap and rinse with clean water to remove all traces of soap, remove all loose flaking paint and repair any cracks and defects, spot prime bare and repaired apply one coat sealer One coat primer, one under coat  and two coats PRASA Neutral"]
[]
[6,"On internal walls",null,"m²",1000]
[]
[null,"Wash with polycell sugar soap and rinse with clean water to remove all traces of soap, remove all loose flaking paint and repair any cracks and defects, spot prime bare and repaired areas with bonding liquid and apply one coat sealer and two coats of white Professional Superior Low Sheen  "]
[]
[7,"On ceiling",null,"m²",250]
[]
[null,"PLATFORM MARKING"]
[]
[null,"Prepare and paint yellow road marking paint on tared platform surfaces"]
[]
[8,"100mm wide yellow line",null,"m",3000]
[]
[{"$nulls":4},"Carried to final summary"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
[]
[null,"BILL NO.12"]
[]
[null,"MASONRY"]
[]
[null,"BRICKWORK"]
[]
[null,"20-30MPa Silver-gray Travertine or similar approved Imperial FBX clay face brick, size 222 x 106 x 73mm, manufactured in accordance with SANS 227:2007, bedded and jointed in Class I mortar and pointed with flush vertical, flush horizontal joints, with every 6th horizontal joint to be recessed. Brickwork of NFP bricks in class II mortar"]
[]
[null,"Bricks in Class II mortar"]
[]
[1,"One brick walls ",null,"m²",100]
[]
[null,"Brick reinforcement"]
[]
[2,"230mm wide reinforcement built in horizontal ",null,"m",150]
[]
[3,"Striking and Pointing on face brick work",null,"m²",250]
[]
[{"$nulls":4},"Carried to final summary"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
[]
[null,"BILL NO. 13"]
[]
[null,"PLASTERING"]
[]
[null,"SUPPLEMENTARY PREAMBLES "]
[]
[null,"Preparatory work for textured finishes:"]
[]
[null,"Textured finishes to be applied to plaster (plaster elsewhere )"]
[]
[null,"All surfaces are to be inspected and approved by Prasa representative before any work is commenced with "]
[]
[null,"Price for texture finishes:"]
[]
[null,"Prices are to include for all priming, preparatory work, etc"]
[]
[null,"One coat wood trowelled smooth cement plaster on brickwork"]
[]
[1,"On walls",null,"m²",150]
[]
[2,"On narrow widths",null,"m²",25]
[]
[null,"EXTERNAL PLASTER"]
[]
[3,"On walls",null,"m²",400]
[]
[4,"On narrow widths",null,"m²",25]
[]
[null,"(4:1) Cement screed to concrete floors "]
[]
[5,"25mm Thick screed to horizontal surfaces to receive ceramic tiles.",null,"m²",50]
[]
[{"$nulls":4},"Carried to final summary"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
[]
[null,"BILL NO. 14"]
[]
[null,"BLINDS"]
[]
[null,"Vertical blinds with 90mm slat width, colour to match walls and floor tiling"]
[]
[1,"Blinds to fit 2 x 2m high opening",null,"No.",10]
[]
[{"$nulls":4},"Carried to final summary"]
[]
[]
[]
[]
[]
[null,"CIVIL AND MINOR GENERAL WORKS FINAL SUMMARY"]
[]
[]
[null,"Desctription",null,"Bill No.",{"$nulls":3},"Amount"]
[]
[]
[1,"Alterations",null,1,{"$nulls":3},"R"]
[]
[2,"Earth works",null,2,{"$nulls":3},"R"]
[]
[3,"Concrete works",null,3,{"$nulls":3},"R"]
[]
[4,"Roof covering",null,4,{"$nulls":3},"R"]
[]
[5,"Carpentry and Joinery",null,5,{"$nulls":3},"R"]
[]
[6,"Ceiling work",null,6,{"$nulls":3},"R"]
[]
[7,"Ironmongery",null,7,{"$nulls":3},"R"]
[]
[8,"Plumbing work",null,8,{"$nulls":3},"R"]
[]
[9,"Metal work",null,9,{"$nulls":3},"R"]
[]
[10,"Glazing",null,10,{"$nulls":3},"R"]
[]
[11,"Paint work",null,11,{"$nulls":3},"R"]
[]
[12,"Masonry",null,12,{"$nulls":3},"R"]
[]
[13,"Plastering",null,13,{"$nulls":3},"R"]
[]
[14,"Blinds",null,14,{"$nulls":3},"R"]
[]
[]
[]
[]
[null,"SUB TOTAL",{"$nulls":5},"R"]
[]
[null,"ADD VAT @ 15%",{"$nulls":5},"R"]
[]
[null,"TOTAL TENDER AMOUNT",{"$nulls":5},"R"]
{"$rows_empty":11}
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
[]
[null,"SECTION No. 3"]
[]
[null,"ELECTRICAL WORKS: SCHEDULE OF QUANTITIES"]
[]
[null,"PROVISIONAL SCHEDULE OF QUANTITIES "]
[]
[null,"Major Supply and Installation of Platform and Shelter Lighting at Tshiawelo Station"]
[]
[null,"BILL NO. 1"]
[]
[null,"ALTERATIONS (PROVISIONAL)"]
[]
[null,"REMOVAL OF EXISTING WORK"]
[]
[null,"Taking out and removing electrical work"]
[]
[1,"400W HPS fittings",null,"No.",6]
[]
[2,"Bulkhead fittings",null,"No.",50]
[]
[3,"4/5 foot fluorescent fittings",null,"No.",35]
[]
[{"$nulls":4},"Carried to final summary"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
[]
[null,"BILL NO.2"]
[]
[null,"ELECTRICAL WORK"]
[]
[null,"Supply, install test commission and hand over"]
[null,"in good working conditions complete the"]
[null,"electrical system as per BoQ, specifications, IEE wiring regulations & as required by Local Electrical Authorities (NEC) for the complete project all up to the Satisfaction of the Engineer. All the material to be supplied to bear SABS mark or SABS mark of compliance."]
[]
[null,"Fluorescent fittings waterproofed fixture white including 2x58w T8 LED Fluorescent tubes and polycarbonate base with clear polycarbonate cover IP65"]
[]
[1,"Waterproof polycarbonate LED 5ft 2 x58w T8 fluorescent fitting including 2 LED tubes",null,"No.",35]
[]
[2,"1200m (4 foot) 2x36w Open channel cool white LED Fluorescent fittings double tubes for ticket office building",null,"No.",25]
[]
[null,"Bulkhead fittings"]
[]
[3,"Corrosion resistance high pressure die- cast aluminium  LED 19w Bulkhead fitting with wire guard IP 65 bearing the SABS Mark minimum 50 000hrs lifetime 4 000K at a colour rendering index >70, injection moulded high impact acrylic diffuser  including opening tool for platform shelters",null,"No.",35]
[]
[null,"High colour rendering index CRI > 80, Colour temperature 4000K, 4710 lumens220-240V LED Module, -25 +800C, LM6 High pressure die cast aluminium body, Borosilicate dlear tempered glass, 316 stainless steel screws and heli-coils, 3 x 20mm diameter entry knockouts and 1 x M20 treaded gland entry"]
[]
[4,"410mmL x 271mmW x 120mmH B40 53W Bulkhead fitting, IP 65 bearing the SABS Mark minimum, 50 000hrs lamp service life, 50000hrs ECG Average life LM6 High pressure die cast aluminium body with high impact polycarbonate diffuser  LED Bulkhead fittings",null,"No.",20]
[]
[5,"7w LED bulk head  fittings completely with bulbs",null,"No.",15]
[]
[null,"HIGH BAY LED FITTINGS"]
[]
[null,"279W LED Lumminaire (34460 lumen) with 3 an optical compartment with LED engine, glass protector, LED warm light with colour temperature of 3000 kelvin, gear compartment and a spigot top entry adjustable compartment. Both optical and gear compartments to be rated IP 66. 20kV/kA surge protection. The luminaire housing to be manufactured of marine grade cast aluminium (EN 1706 AC-44300). Including 1 opening tool"]
[]
[null,"The use of cherry picker/scaffolder or any other equipment to be used for replacing of masts pole fittings and bulbs for the duration of the project"]
[]
[]
[6,"389 x 389 x 168mm 203W LED Lumminaire 32260 lumen) compartment with LED engine, glass protector, LED neutral white 740 with colour temperature of 4000 kelvin, Both optical and gear compartments to be rated IP 66. 10kV/kA surge protection. The luminaire housing to be manufactured of Marine grade high pressure die cast aluminium (EN 1706 AC 44300) optical housing Eco bay fittings to bears the SANS 60598 safety mark",null,"No.",5]
[]
[null,"High mast pole street light fitting"]
[]
[7,"279W LED Lumminaire (34460 lumen) with 3 an optical compartment with LED engine, glass protector, LED warm light with colour temperature of 3000 kelvin, gear compartment and a spigot top entry adjustable compartment. Both optical and gear compartments to be rated IP 66. 20kV/kA surge protection. The luminaire housing to be manufactured of marine grade cast aluminium (EN 1706 AC-44300). Including 1 opening tool",null,"No.",6]
[]
[8,"835x 345 x 35cm 265W LED MAXI light Lumminaire 43584 lumen)  with LED engine, glass protector, LED warm light with 730 colour temperature of 3000 kelvin, gear compartment and a spigot top entry adjustable compartment. Both optical and gear compartments to be rated IP 66. 20kV/kA surge protection. The luminaire housing to be manufactured of marine grade cast aluminium (EN 1706 AC-44300). Including 1 opening tool",null,"No.",18]
[]
[null,"SWITCHES"]
[]
[9,"Day light switches  ",null,"No.",4]
[]
[10,"11 kw contactors",null,"No.",3]
[]
[11,"White 1 lever 2 way switch",null,"No.",15]
[]
[12,"White 2 lever 1 way switch",null,"No.",6]
[]
[null,"Electrical cables"]
[]
[13,"70mm2 4 core armored cable in trenches measured else where  ",null,"m",100]
[]
[14,"25mm2 4 core armored cable in trenches measured else where  ",null,"m",450]
[]
[15,"16mm2 4 core armored cable in trenches measured else where  ",null,"m",300]
[]
[16,"10mm2 4 core armored cable in trenches measured else where  ",null,"m",500]
[]
[17,"4mm2 4 core armored cable in trenches measured else where  ",null,"m",150]
[]
[18,"2.5mm2  GP wires (Red, white, blue, black and earth) for lights rewiring of  shelters in 3 phase system",null,"m",400]
[]
[19,"2.5mm2 suffix cable or GP wire ",null,"m",200]
[]
[20,"1.5mm2 suffix cable or GP wire for lights",null,"m",200]
[]
[null,"Electrical casing"]
[]
[21,"20mm galvanized SABS conduit completely with all the couplings, galvanized saddle, spacer bar assembly and heavy duty U clamps completely encased 100mm deep on concrete walls and make good  ",null,"m",250]
[]
[22,"20mm PVC SABS conduit completely with all the couplings, saddle, spacer bar assembly and heavy duty U clamps",null,"m",100]
[]
[23,"40 x 25mm white heavy duty PVC trunking comlpetely with all the fittings",null,"m",50]
[]
[24,"76 x 76 X 0.8 mm galvanized  heavy duty steel trunking comlpetely with all the fittings",null,"m",30]
[]
[null,"PLUGS"]
[]
[25,"4 x 4 Double plug",null,"No.",10]
[]
[26,"4 x 4 single plug",null,"No.",10]
[]
[null,"Circuit breakers "]
[]
[27,"10 A 1P 6KA single circuit breaker",null,"No.",20]
[]
[28,"10 A 3P 6KA circuit breaker",null,"No.",5]
[]
[29,"12 A 3P Contactor",null,"No.",2]
[]
[30,"20 A 1P 6KA single circuit breaker",null,"No.",25]
[]
[31,"20 A 3P 6KA circuit breaker",null,"No.",3]
[]
[32,"30 A 1P 6KA circuit breaker",null,"No.",3]
[]
[33,"30 A 2P 6KA circuit breaker",null,"No.",3]
[]
[34,"40 A 2P 6KA circuit breaker",null,"No.",3]
[]
[35,"60 A 3P AC1 Contactor",null,"No.",2]
[]
[36,"63 A 2P 6KA circuit breaker",null,"No.",2]
[]
[37,"63 A 3P 6KA circuit breaker",null,"No.",2]
[]
[38,"63 A 30Ma 3P + N Earth leakage",null,"No.",2]
[]
[39,"400 A 3P Main circuit breaker",null,"No.",1]
[]
[40,"250 A 3P Main circuit breaker",null,"No.",2]
[]
[41,"80 A 3P Main circuit breaker",null,"No.",1]
[]
[42,"60 A 3P Main circuit breaker",null,"No.",1]
[]
[43,"40 A stove Isolator",null,"No.",1]
[]
[44,"30A Air conditioner  Isolator",null,"No.",2]
[]
[null,"DB BOARDS"]
[]
[45,"Surface mounted  min distribution board for staffroom (4 offices, one kitchen and 2 separate toilets )completely with circuit breakers",null,"No.",4]
[]
[46,"1000h x 400w x 400d x 2.0mm stainless steel orange IP 65 weatherproofed floor mounted lockable Station kiosk with 1 door completely rewired with all the circuit breakers mounted on din rail as per above and all other accessories, connected to the station",null,"No.",1]
[]
[47,"Lockable fiber glass water proofed 12 way CBI DB  Eaves box to be mounted on external walls for platform shelters, waiting areas, access point, ablutions, etc",null,"No.",15]
[]
[null,"HVAC Systems"]
[]
[48,"Supply, install and commission new 24000 BTU split unit, inverter technology air conditioner completely with all accessories (drain pipe, amorflex, copper pipe, refrigerant, cable, communication wire, brackets, circuit breaker, isolator, etc )",null,"No.",3]
[]
[null,"PLATFORM/STREET HIGH MAST STEEL POLES"]
[]
[null,"Pricing shall includes the design, supply, delivery to site, off-loading, erection, installation, commissioning, testing, and handing over in full working order a high mast lighting structure, including floodlight luminaries."]
[]
[null," The works specifically include the following: "]
[]
[null,"1. Geotechnical studies of proposed sites and issuing of soil test results. "]
[]
[null,"2. Design, preparation and cast of appropriate foundations. "]
[]
[null,"3. Design, supply, delivery to site, off-loading, erection, installation, commissioning, testing, and handing over in full working order a 30 meter high mast pole complete with Luminaries and control panel as specified."]
[]
[null,"4. Perform an electrical connection to the installation from the station kiosk"]
[]
[null,"5. Test and commissioning of the high mast lighting installation. "]
[]
[null,"6. Issuing of a certificate of compliance (COC) in terms of SANS 0142 Code of Practice.  "]
[]
[null,"7. all works should be accordance with the relevant specified specification (wirireing code SANS 0225)"]
[]
[null,"8. 30m high mast light shall be operated and maintaned in the horizontal position by means of a mechanical a mechanical winch "]
[]
[null," Tests "]
[]
[49,"Soil geotechnical studies for foundation including soil and concrete cube tests. ",null,"Per Pole",2]
[]
[50,"Perform soil bearing pressure tests for each mast prior to casting the concrete base to ensure that the soil load bearing conditions are suited to the specific concrete base design. Provide soil test Certificate ",null,"Per Pole",2]
[]
[51,"Test earth system and provide test certificate ",null,"Per Pole",2]
[]
[null,"Earth works"]
[]
[52,"Concrete foundation for high mast complete as per manufactrures specifications with excavation not exceeding 2m deep, steel reinforcing, cables inlet pipes, earth spikes, foundation bolts and template set, back fill material and soil concrete test.",null,"Per Pole",2]
[]
[null,"The use of Crane during the installation of 30m high mast poles"]
[]
[53,"Supply and deliver to site 30m above the ground HDG galvanized street pole with 9way Spiggot to recieve 9 lights per pole, LED Street lights priced elsewhere. Assemble and Erect complete with all accessories, distribution board, internal cables, carriage, earthing with 2 x earth spikesetc.  ",null,"No.",2]
[]
[null,"DOUBLE DRUM WORM WINCH "]
[]
[null,"H:328 MM, W:410mm, M:80kg "]
[]
[null,"Dymot DD800W Double drum Worm Winch "]
[]
[null,"S.W.L.: 800kg   (400kg +400kg) "]
[]
[null,"Rope DIA:6mm "]
[]
[null,"Drum Rope Capacity: 33m "]
[]
[null,"Gear Ratio:  50:1 "]
[]
[null,"Handle Radius:   285 "]
[]
[null,"Swive Base "]
[]
[null,"dia (7x19) Stainless Steel Rope Sling,  33 long "]
[]
[null,"C/W Stainless Thimble & Copper Ferule one end only. "]
[]
[null,"Power Tool "]
[]
[null,"220V Electric Power Tool "]
[]
[null,"c/w Torgue limiter & 3m remote cable "]
[]
[54,"Double Drum Worm Winch completely including, remote, Swive Base, power tools etc used for for lowered of high mast poles ",null,"No.",1]
[]
[null,"PIPE JACKING UNDER RAILWAY LINE"]
[]
[null,"HORIZONTAL DIRECTIONA DRILLING UNDER RAILWAY LINE AND INSTALLATION OF HDPE PIPE"]
[]
[55,"HDD under the railway lines and installation of 110mm diameter HDPE but welded on sleeve pipe with Nominal Pressure class 16 and material of PE100 to be used  including all fittings completely installed ",null,"m",100]
[]
[null,"SLEEVE"]
[]
[56,"110mm HDPE double wall corrugated coil with 5mm plain galvanized draw wire per sleeve. Both ends to be plugged before backfilling",null,"m",800]
[]
[null,"EARTHING"]
[]
[57,"Earth bonding (water pipes, stoves, etc)for the whole station as per SANS 10142 and"]
[null,"the specification.",null,"Item",1]
[]
[null,"ELECTRICAL COMPLIANCE"]
[]
[null,"All work to comply to SANS 10142"]
[null,"Compliance certificate to be provided on completion"]
[null,"Pricing to include all necessary complete connection"]
[]
[58,"Certificate of compliance and all other testing required including 12 month guarantee certificate"]
[]
[{"$nulls":4},"Carried to final summary"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
[]
[null,"BILL NO. 3"]
[]
[null,"EARTHWORKS"]
[]
[null,"EXCAVATION, FILLING, ETC"]
[]
[1,"Removing and relaying of paving blocks after cables has been laid. To be relayed as per manufactures specification",null,"m²",750]
[]
[null,"Excavation in earth not exceeding 2m deep"]
[]
[null,"Trenches"]
[]
[null,"Earth filing obtain from the excavation and/or prescribed stock piles on site compacted to 90% Mod AASHTO density"]
[]
[2,"Backfilling to holes after concrete has been laid ",null,"m3",700]
[]
[null,"15 Mpa/20 mm unreinforced concrete"]
[]
[3,"1m long * 0.5m wide  x 0.2m thick Concrete block on every five meter interval on top of 16 mm² 4-core underground cable",null,"m3",20]
[]
[null,"Tar resurfacing"]
[]
[4,"Cutting of tar, Site preparations and apply 40mm thick Medium Hot Asphalt  ",null,"m²",500]
[]
[{"$nulls":4},"Carried to final summary"]
[]
[]
[]
[]
[]
[]
[null,"FINAL SUMMARY "]
[null,"ELECTRICAL WORK AT TSHIAWELO STATION"]
[]
[]
[null,"SECTION No.3"]
[]
[1,"ALTERATIONS",null,"BILL No.1",{"$nulls":3},"R"]
[]
[2,"ELECTRICAL WORK",null,"BILL No.2",{"$nulls":3},"R"]
[]
[3,"EARTHWORKS",null,"BILL No.3",{"$nulls":3},"R"]
[]
[]
[]
[]
[]
[null,"SUB TOTAL",{"$nulls":5},"R"]
[]
[null,"ADD VAT @ 15%",{"$nulls":5},"R"]
[]
[null,"TOTAL TENDER AMOUNT",{"$nulls":5},"R"]
[]
[]
[]
[]
[]
[]
[null,"FINAL SUMMARY "]
[null,"STATION REFURBISHMENT AT TSHIAWELO STATION"]
[]
[]
[]
[]
[1,"PRELIMINARY AND GENERAL ",null,"SECTION No.1",{"$nulls":3},"R"]
[]
[2,"CIVIL AND GENERAL BUILDING WORK AT MIDWAY STATION",null,"SECTION No.2",{"$nulls":3},"R"]
[]
[3,"ELECTRICAL WORK",null,"SECTION No.3",{"$nulls":3},"R"]
[]
[]
[]
[]
[null,"SUB TOTAL",{"$nulls":5},"R"]
[]
[null,"ADD VAT @ 15%",{"$nulls":5},"R"]
[]
[null,"TOTAL TENDER AMOUNT",{"$nulls":5},"R"]

{"sheet":"LENZ","index":1,"n_rows":1207,"n_cols":8,"rows_kept":1207,"merged":[[0,0,0,1],[7,0,7,1],[32,4,32,6],[156,3,156,5],[185,3,185,5],[210,3,210,5],[238,3,238,5],[309,4,309,6],[365,4,365,6],[419,4,419,6],[616,4,616,6],[647,4,647,6],[672,4,672,6],[757,4,757,6],[780,4,780,6],[816,4,816,6],[828,4,828,6],[871,1,871,5],[873,1,873,5],[875,1,875,5],[912,4,912,6],[1129,4,1129,6],[1155,4,1155,6],[1176,1,1176,5],[1178,1,1178,5],[1180,1,1180,5],[1202,1,1202,5],[1204,1,1204,5],[1206,1,1206,5]],"flags":["formulas_cached_only"]}
[]
[]
[null,"SCHEDULE OF QUANTITIES "]
[]
[null,"MINOR WORKS AT LENZ STATION"]
[]
[null,"CIVIL AND GENERAL BUILDING WORK AT LENZ STATION: RFQ NO:13/07/2022/06CRES"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
["No"]
[null,"SECTION No. 1"]
[]
[null,"BILL NO. 1"]
[]
[null,"PRELIMINARY AND GENERAL "]
[]
[null,"Preliminary and General"]
[]
[1,"All Preliminary and General applicable to this project",null,"Sum",1]
[]
[null,"Occupational Health and safety"]
[]
[null,"The contractor shall comply with all the requirements set out in the Construction Regulations, issued under The Occupational Health & Safety Act no 85 of 1993."]
[]
[null,"Safety file shall be provided by the contractor prior to commencement of work."]
[]
[null,"The contractor shall carry out the works with as little noise and mess as possible. All rubble shall be taken away from site on a daily basis."]
[]
[null,"Note: All designated items should comply with local content threshold. "]
[]
[2,"Compliance with Occupational Health and Safety Act (Act 85 of 1993) and its regulations and with the Employers Health and Safety",null,"Sum",1]
[]
[{"$nulls":4},"Carried to final summary"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
["No."]
[null,"SECTION NO. 2"]
[]
[null,"CIVIL AND GENERAL BUILDING WORK AT LENZ STATION"]
[]
[null,"BILL NO. 1 "]
[]
[null,"ALTERATIONS  "]
[]
[null,"SUPPLEMENTARY PREAMBLES  "]
[]
[null,"General "]
[]
[null,"Special care shall be exercised during the progress of the"]
[null," work to ensure that any electrical installations, water supply"]
[null," pipes, telephone and other services which may be"]
[null," encountered are not interfered with and notice shall be given"]
[null," to the project manager if any disconnection or"]
[null," alterations become necessary"]
[]
[null,"The contractor shall take all precautions necessary to"]
[null," prevent any nuisance from dust whilst carrying out the work"]
[]
[null,"Leave in good condition"]
[]
[null,"The contractor must leave the existing building,in which "]
[null,"the alterations are executed ,clean and neat at completion"]
[]
[null,"Price shall include removal and disposal of rubble from site"]
[]
[]
[null,"REMOVAL OF EXISTING WORK  "]
[]
[]
[null,"Taking down and removing ceiling"]
[]
[1,"Suspended ceiling",null,"m²",50]
[]
[null,"Rhino Board ",null,"m²",300]
[]
[null,"Taking down and removing doors"]
[]
[2,"Timber single door 813 x 2032",null,"No.",10]
[]
[]
[null,"Taking out and removing glass, beads, etc"]
[]
[3,"Brocken window pane from steel frame including upgrading, cleaning and preparation to receive new",null,"m²",15]
[]
[null,"Taking out and removing roofs"]
[]
[4,"Asbestos roof",null,"m²",200]
[]
[null,"Hacking up/off and removing ceramic tile floor and wall finishes including removing mortar bed or backing and preparing concrete or brick surface for new screed, plaster or tile finishes"]
[]
[5,"150 x 150mm tiles to walls",null,"m²",50]
[]
[6,"300 x 300mm tiles to floors",null,"m²",50]
[]
[null,"Taking out and removing piping, sanitary fittings, etc including disconnection piping from fittings"]
[]
[7,"9l Ceramic pan and cistern ",null,"m²",15]
[]
[8,"wash hand basin including all fittings",null,"No",7]
[]
[9,"Down pipes",null,"m",200]
[]
[10,"Gutters",null,"m",80]
[]
[null,"Taking out, removing, upgrading and re-installation"]
[]
[11,"Steel palisade fencing by cutting 1m of the bottom rusted part of the main poles, supply and weld 1m High 65 x 65mm new pole to match existing, apply anticorrosion coating and installation of fencing on concrete footings  including welding of removed 3m steel palisade panels and painting with Prasa colours   ",null,"m",350]
[]
[null,"Taking out and removing"]
[]
[12,"2000 x 2000mm high blinds",null,"No",15]
[]
[null,"SERVICING, REPAIRING, RE-FIXING, CLEANING, ETC OF EXISTING WORK"]
[]
[null,"Clean down existing roof sheeting, box gutters, flashings. Etc apply de-rusting compound to surfaces, prepare area for paint application and allow for re-fixing, replacing and waterproofing of necessary roof screws, fixing screws, etc"]
[]
[13,"IBR roof sheeting in fair condition not exceeding 30 degree slope",null,"m²",60]
[]
[14,"Sheet steel box gutters in fair condition",null,"m",200]
[]
[null,"Re-fixing and aligning of fascia and barge boards"]
[]
[15,"Fibre cement fascia and barge boards not exceeding 300mm girth",null,"m",50]
[]
[16,"Sheet metal fascia and barge boards not exceeding 300mm girth",null,"m",50]
[]
[null,"Clean down existing facebrick façade, painted walls, plinths, wall tiles, floor tiles, etc with water and brush "]
[]
[17,"Internal and external face brick walls",null,"m²",500]
[]
[18,"Internal ceramic wall and floor tiles",null,"m²",200]
[]
[null,"Clean down existing window panes"]
[]
[19,"Glazing to steel windows measured on both sides",null,"m²",100]
[]
[null,"Clean out existing roofs"]
[]
[20,"High pressure jetting and cleaning to roofs ",null,"m²",2000]
[]
[null,"Clean out and service gutters"]
[]
[21,"125 x 100mm eaves gutter",null,"m",100]
[]
[22,"250 x 200mm industrial eaves gutter",null,"m",100]
[]
[null,"Upgrading of stormwater and Sewer network"]
[]
[23,"High pressure jetting and cleaning of 300mm diameter stormwater underground pipe",null,"m",350]
[]
[24,"High pressure jetting and cleaning of 110mm diameter sewer underground pipe",null,"m",350]
[]
[null,"Taking out and removing manhole covers"]
[]
[25,"600 x 900mm steel manhole frame including surface preparation to receive new",null,"No.",20]
[]
[{"$nulls":3},"Carried to final summary"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
[]
[null,"BILL NO 2"]
[]
[null,"Earthworks (Provisional)"]
[]
[null,"Supplementary Preambles"]
[]
[null,"All soil poisoning and insecticide to be applied under a ten year guarantee by an approved firm of specialist"]
[]
[null,"General notes"]
[]
[null,"Fill material shall be placed in lift of not more than 150mm"]
[null,"Compaction density to be controlled using DCP apparatus to a maximum of 30mm/blow 93% MOD AASHTO compaction is to be achieved "]
[]
[null,"Where backfill is required on both sides of walls, backfill both sides simultaneously."]
[]
[null,"Where compaction of fill material behind retaining walls is done using mechanical rollers, the rollers must be kept 500mm away from the wall and this 500mm portion must be compacted with hand stampers or wackers."]
[]
[null,"Site Clearance"]
[]
[1,"Cleaning and removal of rubble from site",null,"m²",8000]
[]
[null,"G5 Material  compacted to 93% Mod AASHTO density"]
[]
[2,"Backfilling to trenches",null,"m3",400]
[]
[{"$nulls":3},"Carried to final summary"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
[]
[null,"BILL NO 3"]
[]
[null,"CONCRETE WORK"]
[]
[null,"Application: Outdoor Litter Bin"]
[null,"External size: 700mm x 700mm x 875mm high"]
[null,"Internal size: 600mm x 600mm x 700mm deep"]
[null,"Capacity: 320 litres"]
[null,"Mass: 430kg"]
[null,"Finish: Exposed aggregate"]
[null,"Advertising space: 4 x 685mm x 590mm"]
[null,"Drainage hole in bottom"]
[]
[1,"Supply and deliver Advertising Bin with exposed aggregate external finish ",null,"No.",15]
[]
[null,"STEEL BRIDGE TREADS"]
[]
[null,"Reinforced Precast Concrete Bridge Treads"]
[]
[2,"2500mm long x 300mm wide x 80mm deep precast concrete bridge treads as per attached drawing with bending schedule",null,"No.",25]
[]
[{"$nulls":3},"Carried to final summary"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
[]
[null,"BILL NO 4"]
[]
[null,"ROOF COVERING ETC"]
[]
[null,"PROFILE METAL SHEETING AND ACCESSORIES"]
[]
[null,"Roof sheeting to be Concealed Fix interlocking \"KLIP-LOK 700\",  0,58mm thick heavy industrial Z275 spelter galvanised steel sheeting with Chromadek, ColorPlus, Colourbond or Globalcoat finish to one side and Grey other side and accessories, fixed to steel purlins using SL 700  approved clips and fasteners. Cover width 700mm. High wind - 120km/h plus - loading to be considered with installation and fixing must be in accordance with manufacturer's recommendations and specifications."]
[]
[1,"Roof covering with pitch not exceeding 25 degrees",null,"m²",250]
[]
[2,"450mm galvanized steel roll top ridge",null,"m",30]
[]
[null,"REPAIRS TO GALVANISED IRON ROOF COVERING"]
[]
[null,"Carfully examine entire roof area and locate leaks with particular attention"]
[null,"given to roof leaks where marks are available on walls and ceiling.Locate holes"]
[null,"and solder.Replace defective screws using longer screws as ''Reaseal'' or similar"]
[null,"approved as SABS Specification 135 where purlins are fixed on edge,and 6mm "]
[null,"bolts where purlins are fixed on flat.Beat into corrugation damaged or buckled"]
[null,"edges,fix in position where necessary using self tapping screws,roofing screws"]
[null,"or verandah bolts.Similarly examine all flashing,ridging and vally linings,"]
[null,"repair and refix loose sections,as for the roof covering.No plastic or other"]
[3,"compounds are to be used to render leaks watertight.",null,"m²",4000]
[]
[{"$nulls":3},"Carried to final summary"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
[]
[null,"BILL NO. 5"]
[]
[null,"CARPENTRY AND JOINERY  "]
[]
[null,"TIMBER  "]
[]
[null,"All softwood to be South African Pine  "]
[]
[]
[null,"DOORS, ETC"]
[]
[null,"Wrought meranti doors hung to steel frames"]
[]
[null,"44mm thick exterior grade flush solid core timber single door with 3mm thick commercial ply on both sides with consolidated edges fitted and complying with SABS 545 in pressed steel frame. All painted in accordance with architect's colour schedules"]
[]
[1,"813 x 2032 x 44mm single leaf solid core with commercial veneer for paint. pricing shall include painting as per manufactures specification",null,"No.",10]
[]
[null,"44mm thick interior grade flush solid core timber single door with 3mm thick commercial ply on both sides with consolidated edges fitted and complying with SABS 545 in pressed steel frame. All painted in accordance with architect's colour schedules"]
[]
[2,"813 x 2032 x 44mm single leaf solid core with commercial veneer for paint. pricing shall include painting as per manufactures specification",null,"No.",10]
[]
[null,"FITTINGS"]
[]
[null,"The following in modular timber cupboards, counters, duty stations, desk etc. as per Cupboard Connections Specification"]
[]
[null,"Carcasses of 16mm thick particle board with both faces white melamine with white Masonite backs. Shelving of 16mm particle board, both faces white melamine and front edge in white PVC. Doors of 16mm particle board with post formed vertical edges and laminated in Renolit. Tops of 32mm particle board with post formed leading edges and laminated in high pressure decorative laminate. All butt edges and edges against walls to be sealed with silicon sealant. Hinges to be “Hettich”. Drawer runners to be metal 500mm series with nylon runners or similar. All units complete with door, handles, hinges, cupboards, door, locks, barrel bolts and shelves. Floor unit complete with kick plates. (Formica tops measured elsewhere)   "]
[]
[null,"Built in cupboards fittings"]
[]
[null,"General"]
[]
[null,"The following cupboard fittings have been measured as complete units i.e. the components of the units have not been separately measured. The descriptions, therefore, of such units shall be deemed to include all components, assembling, housing, notching, glueing, blocking, planting on and screwing with countersunk screws, edge strips, decorative plastic finish, glass, ironmongery, metalwork and paint or varnish finishes"]
[]
[null,"Kitchen cupboards,etc."]
[]
[3,"Kitchen sink floor cupboard 2000 x 600 x 900mm high with sides, bottom, back, 3 hinged doors and one drawer completely working including handles, etc. top and sink measured else where",null,"No.",1]
[]
[null,"Interior type particle board with Formica veneer "]
[]
[4,"900 x30mm thick granite with all exposed edges large bevel edged, fixed to supports using dabs of 100% black silicone adhesive along all supports with all joints filled with matching polyester resin glue. Granite surface to be sealed using an approved stone sealer, all in accordance with the manufacturer's recommendations.",null,"m",4]
[]
[5,"2mm thick edge strip 32mm wide",null,"m",6]
[]
[6,"Cut 50mm work top to fit end bowl sink, measured else where ",null,"No.",1]
[]
[null,"EAVES, VERGES, ETC"]
[]
[null,"Pressed fibre cement"]
[]
[7,"10 x 225mm Fascia’s including galvanized steel H-Profile jointing strips",null,"m",60]
[]
[8,"10 x 230mm Barge boards including galvanized steel H-profile jointing strips ",null,"m",25]
[]
[null,"Wrought softwood "]
[]
[9,"50 x 75mm purlins at 900mm center’s to sides of trusses ",null,"m",60]
[]
[10,"38mm x 114mm wall plates ",null,"m",30]
[]
[11,"38mm x 100mm Grade M4 ridge beam",null,"m",30]
[]
[12,"50mm x 75mm purlins",null,"m",60]
[]
[null,"Sundries"]
[]
[13,"Two coats creosote on sawn timbers",null,"m²",80]
[]
[{"$nulls":4},"Carried to final summary"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
[]
[null,"BILL NO 6"]
[]
[null,"CEILING WORK"]
[]
[null,"SUPPLEMENTARY PREAMBLES "]
[]
[null,"Description "]
[]
[null,"Items described as “nailed” shall be deemed to be fixed with hardened steel nails or pins or shot pinned to brickwork or concrete"]
[]
[null,"Items described as “plugged” shall be deemed to include screwing to fibre, plastic or metal plugs at not exceeding 600mm centres, and where described as “bolted”, bolts priced elsewhere"]
[]
[null,"Finishes to suspended ceilings:"]
[]
[null,"All finishes to be applied at the factory during the manufacturing process and to be delivered on site “pre-finished” as described. No applying of finishes on site will be allowed"]
[]
[null,"NAILED UP CEILING"]
[]
[null,"6mm “Everite Nutec” fibre cement boards with H-type pressed steel jointing including painting with one coat of alkali resistance primer , one undercoat and two coat eggshell enamel paint"]
[]
[1,"ceiling generally 600mm wide including 38 x 38mm sawn softwood brandering at maximum 600mm centres nailed to and including 75 x 50mm sawn softwood bearers at 900mm centres suspended approximately 250mm below timber trusses with 75 x 38mm vertical bearers at 600mm centres nailed to tie beams of trusses",null,"m²",200]
[]
[2,"Extra over ceiling for 800 x 800mm trap door of 38 50mm wrought softwood rebated framing with one 38 x 38mm sawn softwood cross brander covered with ceiling board and fitted flush in opening",null,"No.",3]
[]
[null,"“Rhino” gypsum plasterboard cornice"]
[]
[3,"75mm coved cornices fixed to ceiling",null,"m",250]
[]
[null,"SUSPENDED CEILING"]
[]
[null,"OWAcoustic(R) Futura Premium biologically absorbable mineral wool ceiling tiles, NRC - 0.75, size 1200 x 600 x 15mm with Square-edge and white painted finish, laid on fire rated OWAconstruct(R) system S3 exposed demountable  T24 suspension system, comprising galvanised main tees and cross tees with main tees suspended by means of galvanised hangers at centres not exceeding 1200mm with ceiling perimeter finished with OWAconstruct Shadowline W-trim, plugged and screwed at 200mm centres, and all installed to manufacturer's instructions."]
[]
[4,"Suspended ceiling not exceeding 1m below concrete soffit",null,"m²",70]
[]
[null,"Cornices to suspended ceiling"]
[]
[5,"Standard brilliant white pre-painted metal angle cornices plugged",null,"m",100]
[]
[null,"PARTITIONS"]
[]
[null,"Lafarge Gypsum or similar approved fixed partition drywall partitioning system with an overall thickness of 89mm comprising internal framing formed of 64mm galvanised steel studs fixed at 600mm centres to galvanised steel track or female aluminium head section and galvanised steel floor tracks including where necessary any additional galvanised steel studding to form door openings, glazing and other apertures, angles, corners and termination ends. Internal steel framing to be dressed on both sides with 12mm thick tapered edge Lafarge or similar approved plasterboard in single lengths to suite height, butt jointed and secured to steel studding with 25mm drywall screws at 220mm centres, joints to be tapped and jointed with Lafarge or similar approved Jointing Compound and prepared for decoration. All exposed aluminum door frames, glazing frames, ceiling and wall channels, battens and skirting are to be formed of natural anodised aluminium sections. Installation to be in accordance with SABISA installation guidelines."]
[]
[6,"Partitioning 3000mm high with bottom track plugged and top track fixed to ceiling including 75mm anodized aluminium skirting fixed to both sides of partitioning",null,"m",100]
[]
[7,"Extra over partitioning 3000mm high for vertical abutment ",null,"No",30]
[]
[8,"Extra over partitioning 3000mm high for corner",null,"No",16]
[]
[9,"Extra over partitioning 3000mm high for T-intersection",null,"No",10]
[]
[10,"Extra over partitioning 3000mm high for fair end",null,"No",16]
[]
[{"$nulls":4},"Carried to final summary"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
[]
[null,"BILL NO 7"]
[]
[null,"IRONMONGERY"]
[]
[null,"LOCKS"]
[]
[null,"Supply and install"]
[]
[1,"Ultra-security heavy duty double pin locks",null,"No",10]
[]
[2,"3 liver mortice lockset with handles",null,"No",30]
[]
[3,"Indicator door lock chrome plated",null,"No",15]
[]
[4,"90mm square Padlock",null,"No",4]
[]
[null,"BATHROOM FITTINGS  "]
[]
[5,"Satin stainless-steel toilet roll holders for 2 rolls with central shaft system and cylinder lock, plugged and screwed to the wall with stainless steel screws. (vandal resistant)",null,"No",3]
[null," "]
[null,"Door closer"]
[]
[6,"Heavy duty alumminium door closer",null,"No",5]
[]
[null,"SIGNAGE"]
[]
[null,"External signage"]
[]
[null,"Male Signage"]
[]
[7,"500 x 500 x 3mm mild steel ACM panel with vinyl graphic overlay",null,"No",1]
[]
[null,"Female Signage"]
[]
[8,"500 x 500 x 3mm mild steel ACM panel with vinyl graphic overlay",null,"No",1]
[]
[null,"Double Sided Platform Station Name "]
[]
[9,"2100mm x 3000 x 3mm mild steel ACM panel sprayed to Pantone 3005C with vinyl graphic overlay and white vinyl graphics mounted on 65mm diameter x 2.6m high above the ground mild steel poles in concrete footing ",null,"No",3]
[]
[null,"Stainless Steel Grade 304 Platform Public Seating"]
[]
[null,"Arms and Legs: Aluminium Die-Cat, chromed. "]
[]
[null,"Cross beam: 2mm Aluminium extrusion, silver. "]
[]
[null,"Seat and back: Stainless steel "]
[]
[10,"5 Seater 2890mmW x 670mmD x 785mmH Peforated mild steel epoxy coated chairs suitable for outdoors burried on earth less then 1mm deep including excavation, concrete, backfilling, etc",null,"No",10]
[]
[{"$nulls":4},"Carried to final summary"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
[]
[null,"BILL NO 8"]
[]
[null,"PLUMBING WORK "]
[]
[null,"SANITARY FITTINGS"]
[]
[1,"Vandal resistance low level High traffic suite complete (Front flush), suite to includes CC  white Cistern made from high strength technoplast polymer with concealed mounting bracket, heavy duty securing bolts, concealed tamper proof lid screws and hiflo MK3 flush valve, including CC Pan and and heavy duty seat.",null,"No",7]
[]
[2,"Close coupled suite colour White , comprising 90º outlet open rim pan with matching 9 litre front single flush cistern including lid and fitments and Jazz Thermoset seat.",null,"No",7]
[]
[3,"Ceramic wash hand basin colour White, size 510 x 405mm with one tap hole including integrated overflow and chain stay hole bolted to wall with two x 10mm bolts and including Classic floor mounted pedestal and sealed with silicone sealant where basin meets wall.",null,"No",10]
[]
[null,"URINAL BASIN"]
[]
[4,"Sanitary ware white vitreous wall mounted urinal with top inlet or back inlet . Overall size 600x385x380mm. Supplied with 38mm c.p. domical grating, a spreader(with a 20mm tread) and two hanger brackets",null,"No",2]
[]
[5,"1830 x 1220mm high floor mounted curved manual flush urinal Centre outlet manufactured from stainless steel AISI 304 including 20Mpa/20mm for installation and unreinforced concrete slab",null,"No",1]
[]
[null,"SINK, BASIN, ETC"]
[]
[6,"Grade 430 stainless steel double bowl sink and drainer size 1160 x 460mm with tiling key, 40mm chromium plated flanged outlets and waste unions, vulcanite or rubber plugs, chromium plated chains and stays, 40mm rubber resealing P-trap with extension piece and clamped connections",null,"No.",2]
[]
[null,"TAPS, VALVES, ETC"]
[]
[null,"Supply and install"]
[]
[7,"Self-closing push button tap",null,"No.",10]
[]
[8,"15mm chrome plated deck mounted sink mixer with overarm swivel outlet and adjustable flanges, manufactured in accordance with SANS 226:2004 Type 1.",null,"No.",2]
[]
[9,"15mm brass garden  tap ",null,"No.",1]
[]
[10,"Exposed type urinal flush valve with ball-o-stop, wall flange, chrome plate finish and non-hold open feature",null,"No.",2]
[]
[11,"15mm Ø BSP built-in sleeve, DZR brass urinal flush valve with internal flow control, strainer and no-hold feature for single bowl urinal.",null,"No.",1]
[]
[12,"Flexi connector",null,"No",30]
[]
[13,"15 Brass Gate Valve ",null,"No",4]
[]
[14,"15mm Mini Ball Valve ",null,"No",30]
[]
[15,"22mm Brass Gate Valve including cast iron valve box",null,"No",2]
[]
[null,"WASTE UNINON ETC"]
[]
[16,"Basin waste, plug, chain, stay and backnut  ",null,"No.",10]
[]
[null,"TRAPS ETC"]
[]
[17,"38mm sink “P” trap",null,"No.",10]
[]
[18,"365/40 CP bottle trap 40 x 40 INC CP/PVC adaptor to 40mm suitable for wash hand basin and urinal ceramic basin",null,"No.",5]
[]
[19,"110mm pan connector completely ",null,"No.",14]
[]
[null,"WATER SUPPLIERS"]
[]
[null,"Class “O” copper pipe "]
[]
[20,"15mm pipes ",null,"m",20]
[]
[21,"15mm pipes chased into brick walls and make good",null,"m",35]
[]
[22,"22mm pipes ",null,"m",10]
[]
[23,"22mm pipes chased into brick walls",null,"m",10]
[]
[null,"Extra over class “O” copper pipes for capillary fittings"]
[]
[24,"15mm fitting  ",null,"No.",10]
[]
[25,"22mm fitting  ",null,"No.",5]
[]
[26,"15mm Tee",null,"No.",10]
[]
[27,"22mm Tee",null,"No.",5]
[]
[null,"Galvanized pipe "]
[]
[28,"32mm pipes ",null,"m",10]
[]
[null,"Extra over class Galvanized pipes for capillary fittings"]
[]
[29,"32mm fitting  ",null,"No.",3]
[]
[30,"32mm elbow  ",null,"No.",2]
[]
[31,"32mm Tee",null,"No.",2]
[]
[null,"Plastic pipe"]
[]
[32,"75mm high pressure plastic pipes in trenches less than 2m deep",null,"m",50]
[]
[33,"75mm gate valve",null,"No.",1]
[]
[34,"Male adaptor",null,"No.",6]
[]
[35,"Straight coupling",null,"No.",6]
[]
[null,"Plastic waste pipes"]
[]
[36,"50mm waste pipes with all connection and make good",null,"m",50]
[]
[null,"SOIL DRAINAGE"]
[]
[null,"Upvc class 34 pipes including excavation, bedding, backfilling and compaction and disposal of surplus material"]
[]
[37,"110mm pipes laid in and including trenches not exceeding 1m deep",null,"m",50]
[]
[38,"Extra over Upvc class 34 pipes for fittings",null,"No.",6]
[]
[39,"110 Bend",null,"No.",5]
[]
[44,"110mm junction",null,"No.",4]
[]
[41,"110mm Access bend",null,"No.",2]
[]
[null,"Sundries"]
[]
[42,"110mm Upvc cleaning eye to end of 110 Upvc pipe",null,"No.",2]
[]
[43,"350 x 350 x 50mm thick precast concrete inspection eye marker slab finished smooth on exposed surfaces with letters “I.E” or “I.O” on top and placed flush in ground or paving",null,"No.",2]
[]
[44,"Testing soil drainage system ",null,"Item",1]
[]
[null,"WATER RETICULATION"]
[]
[null,"PREAMBLES"]
[]
[null,"The contractor is referred to the General Preambles for trades 2017 published by the Association of South Africa Quantity Surveyors before pricing"]
[]
[null,"WATER PIPEWORK"]
[]
[null,"HDPE PE 100PN 12.5 pipes including excavation, bedding, backfilling, and compaction and disposal of surplus material"]
[]
[null,"High density polyethylene class 16 pipes"]
[]
[45,"25mm pipes with all other required connections laid in and including trenches less then 1m deep",null,"m",100]
[]
[46,"25mm fitting  ",null,"No.",3]
[]
[47,"25mm elbow  ",null,"No.",2]
[]
[48,"25mm Tee",null,"No.",2]
[]
[49,"Testing water supply system ",null,"Item",1]
[]
[null,"PLATFORM MANHOLE COVERS AND FRAMES"]
[]
[]
[50,"Type 9B MD polymer lid and frame including to make good after completion",null,"No.",10]
[]
[51,"600 x 900mm polymer lid and frame including to make good after completion",null,"No.",35]
[]
[null,"ELECTRIC WATER HEATERS"]
[]
[null,"Supply, deliver and install Electrical geysers with all other accessories  "]
[]
[null,"Hydro boiler"]
[]
[52,"5 litre Stainless steel water boiler , with stainless steel tank, steam free boiling water, electronic controls, 15mm overflow, connected to 15mm cold water supply including isolating valve and 230 volt 1800 watt electrical power supply, plugged and screwed to wall and fitted under 1 year warranty.",null,"No.",2]
[]
[null,"RAIN WATER GOODS"]
[]
[null,"0.8mm galvanized sheet iron"]
[]
[53,"125 x 100mm eaves gutter",null,"m",150]
[]
[54,"Extra over 125 x 100mm eaves gutter for stopped end",null,"No.",20]
[]
[55,"Extra over 125 x 100 eaves gutter for angle",null,"No.",25]
[]
[56,"Extra over 125 x 100mm eaves gutter for outlet for 100 x 75mm pipe",null,"No.",20]
[]
[57,"100 x 75mm rainwater pipes",null,"m",70]
[]
[58,"Extra over 100 x 75mm rainwater pipe for shoe",null,"No.",20]
[]
[null,"0.9mm galvanized sheet iron"]
[]
[59,"250 x 200mm industrial eaves gutter including heavy duty brackets fixed at 500mm centers",null,"m",100]
[]
[60,"Extra over 250 x 200mm eaves gutter for stopped end",null,"No.",10]
[]
[61,"Extra over 250 x 200 eaves gutter for angle",null,"No.",5]
[]
[62,"Extra over 125 x 100mm eaves gutter ",null,"No.",10]
[]
[63,"300mm rainwater pipes",null,"m",50]
[]
[64,"Extra over rainwater pipe for shoe",null,"No.",10]
[]
[{"$nulls":4},"Carried to final summary"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
["No."]
[]
[null,"BILL NO.9"]
[]
[null,"METAL WORK"]
[]
[null,"SECURITY GATES "]
[]
[null,"Supply and install Burglar door"]
[]
[1,"900 x 2100mm high Heavy duty Burglar door and frame with 16mm steel round bar and 40 x 40 x 2.5mm square tubing ",null,"No.",5]
[]
[null,"Supply and install Burglar windows"]
[]
[2,"508mm W x 629mm H Box windows guard constructed with 5mm of expanded metal and 50 x 50 x 6mm equal angles.",null,"No.",10]
[]
[null,"Gates"]
[]
[null,"Gates welded to steel footbridge"]
[]
[3,"Supply and Install mild steel welded double swing gate 3m high x 4m wide steel swing gate with heavy duty hinges constructed from 76x50x3.5mm frame, diagonal intermediate steel section of 12x12mm at 100mm centers with heavy duty lock and bullet type hinges completely",null,"No.",2]
[]
[4,"1500mm wide x 2400mm high galvanized steel palisade pedestrian gate and posts including large pad locks on 200mm electro galvanized pad bolt lock welded on the gate",null,"No.",1]
[]
[null,"Razor wire"]
[]
[5,"450mm razor barbed wire mounted on top of fencing",null,"m",350]
[]
[{"$nulls":4},"Carried to final summary"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
[]
[]
[null,"BILL NO.10"]
[]
[null,"GLAZING"]
[]
[null,"GLAZING TO STEEL WITH PUTTY"]
[]
[null,"4mm clear float glass"]
[]
[1,"Panes exceeding 0.1 m2 and not exceeding 0.5m2",null,"m²",20]
[]
[null,"4mm clear obscure glass"]
[]
[2,"Panes exceeding 0.1 m2 and not exceeding 0.5 m2",null,"m²",10]
[]
[null,"Mirrors"]
[]
[null,"6mm silver float glass copper backed mirrors with polished edges holed for and fixed with chromium plated dome capped mirror screws with rubber buffers to plugs in brickwork"]
[]
[3,"Mirror 1000 x 1000mm with four screws",null,"No.",3]
[]
[{"$nulls":4},"Carried to final summary"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
[]
[]
[null,"BILL NO.11"]
[]
[null,"PAINTWORK"]
[]
[null,"For preambles see “Model Preambles for Trades” 2008 edition published by the Association of South African Quantity Surveyors "]
[]
[null,"SUPPLEMENTARY PREAMBLES"]
[]
[null,"Previously painted plastered surfaces "]
[]
[null,"Surfaces shall be thoroughly washed down and allowed to dry completely before any paint is applied. Blistered or peeling paint shall be completely removed and cracks shall be opened, filled with a suitable filler and finished smooth"]
[]
[null,"Previously painted metal surfaces "]
[]
[null,"Surfaces shall be thoroughly rubbed and cleaned down. Blistered or peeling paint shall be completely removed down to bare metal"]
[]
[null,"Previously painted wood surfaces "]
[]
[null,"Surfaces shall be thoroughly cleaned down. Blistered or peeling paint shall be completely removed and cracks and crevices shall be primed, filled with a suitable filler and finished smooth"]
[]
[null,"PAINTWORK, ETC TO NEW WORK"]
[]
[null,"ON FLOATED PLASTER"]
[]
[null,"One coat professional plaster primer and two coats of white Professional Superior Low Sheen  "]
[]
[1,"On ceiling and cornices ",null,"m²",300]
[]
[null,"ON WOOD"]
[]
[null,"One coat wood primer, one Universal Undercoat  and two coats Prasa Oakley Brown enamel paint"]
[]
[2,"On doors ",null,"m²",150]
[]
[null,"ON METAL"]
[]
[null,"One coat zinc chromate primer, one under coat  and two coats professional white gloss enamel paint"]
[]
[3,"On buglers, gates, door frames, window frames, rainwater goods etc",null,"m²",200]
[]
[null,"One coat primer, one under coat  and two coats PRASA Neutral"]
[]
[4,"On Dry wall",null,"m²",600]
[]
[null,"One coat professional plaster primer and two coats contractors Brick and Slasto Dressing/Brick seal"]
[]
[5,"On internal and external face brick walls   ",null,"m²",2000]
[]
[null,"PAINTWORK ETC TO PREVIOUSLY PAINTED WORK"]
[]
[null,"ON METAL"]
[]
[null,"Wash with polycell sugar soap and rinse with clean water to remove all traces of soap, remove all loose flaking paint and repair any cracks and defects, spot prime bare and repaired areas with bonding liquid and apply One coat of waterprime, one coat of universal undercoat, two coats of gloss Enamel of PRASA Grey "]
[]
[6,"On footbridge and all steel work",null,"m²",2000]
[]
[null,"Wash with polycell sugar soap and rinse with clean water to remove all traces of soap, remove all loose flaking paint and repair any cracks and defects, spot prime bare and repaired apply one coat sealer and two coats of PRASA Blue\n\n"]
[]
[7,"On steel palisade measured on both sides",null,"m²",1680]
[]
[null,"Wash with polycell sugar soap and rinse with clean water to remove all traces of soap, remove all loose flaking paint and repair any cracks and defects, spot prime bare and repaired apply one coat sealer and two coats of PRASA Blue\n\n"]
[]
[8,"On roofs",null,"m²",4000]
[]
[null,"ON FLOATED PLASTER"]
[]
[null,"Wash with polycell sugar soap and rinse with clean water to remove all traces of soap, remove all loose flaking paint and repair any cracks and defects, spot prime bare and repaired apply one coat sealer One coat primer, one under coat  and two coats PRASA Neutral"]
[]
[9,"On internal walls",null,"m²",1000]
[]
[null,"Wash with polycell sugar soap and rinse with clean water to remove all traces of soap, remove all loose flaking paint and repair any cracks and defects, spot prime bare and repaired areas with bonding liquid and apply one coat sealer and two coats of white Professional Superior Low Sheen  "]
[]
[10,"On ceiling",null,"m²",250]
[]
[null,"PLATFORM MARKING"]
[]
[null,"Prepare and paint yellow road marking paint on tared platform surfaces"]
[]
[11,"100mm wide yellow line",null,"m",1400]
[]
[{"$nulls":4},"Carried to final summary"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
[]
[]
[null,"BILL NO.12"]
[]
[null,"MASONRY"]
[]
[null,"BRICKWORK"]
[]
[null,"20-30MPa Silver-gray Travertine or similar approved Imperial FBX clay face brick, size 222 x 106 x 73mm, manufactured in accordance with SANS 227:2007, bedded and jointed in Class I mortar and pointed with flush vertical, flush horizontal joints, with every 6th horizontal joint to be recessed. Brickwork of NFP bricks in class II mortar"]
[]
[null,"Bricks in Class II mortar"]
[]
[1,"One brick walls ",null,"m²",150]
[]
[null,"Brick reinforcement"]
[]
[2,"230mm wide reinforcement built in horizontal ",null,"m",150]
[]
[3,"Striking and Pointing on face brick work",null,"m²",300]
[]
[{"$nulls":4},"Carried to final summary"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
[]
[null,"BILL NO. 13"]
[]
[null,"PLASTERING"]
[]
[null,"SUPPLEMENTARY PREAMBLES "]
[]
[null,"Preparatory work for textured finishes:"]
[]
[null,"Textured finishes to be applied to plaster (plaster elsewhere )"]
[]
[null,"All surfaces are to be inspected and approved by Prasa representative before any work is commenced with "]
[]
[null,"Price for texture finishes:"]
[]
[null,"Prices are to include for all priming, preparatory work, etc"]
[]
[null,"One coat wood trowelled smooth cement plaster on brickwork"]
[]
[1,"On walls",null,"m²",200]
[]
[2,"On narrow widths",null,"m²",25]
[]
[null,"EXTERNAL PLASTER"]
[]
[3,"On walls",null,"m²",200]
[]
[4,"On narrow widths",null,"m²",25]
[]
[null,"(4:1) Cement screed to concrete floors "]
[]
[5,"25mm Thick screed to horizontal surfaces to receive ceramic tiles.",null,"m²",50]
[]
[{"$nulls":4},"Carried to final summary"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
[]
[null,"BILL NO. 14"]
[]
[null,"BLINDS"]
[]
[null,"Vertical blinds with 90mm slat width, colour to match walls and floor tiling"]
[]
[1,"Blinds to fit 2 x 2m high opening",null,"No.",13]
[]
[{"$nulls":4},"Carried to final summary"]
[]
[]
[]
[]
[]
[null,"CIVIL AND MINOR GENERAL WORKS FINAL SUMMARY"]
[]
[null,"MINOR WORKS AT LENZ STATION"]
[]
[null,"Desctription",null,"BILL",{"$nulls":3},"Amount"]
[]
[null,"SECTION 2"]
[]
[1,"Alterations",null,1,{"$nulls":3},"R"]
[]
[2,"Earth works",null,2,{"$nulls":3},"R"]
[]
[3,"Concrete works",null,3,{"$nulls":3},"R"]
[]
[4,"Roof covering",null,4,{"$nulls":3},"R"]
[]
[5,"Carpentry and Joinery",null,5,{"$nulls":3},"R"]
[]
[6,"Ceiling work",null,6,{"$nulls":3},"R"]
[]
[7,"Ironmongery",null,7,{"$nulls":3},"R"]
[]
[8,"Plumbing work",null,8,{"$nulls":3},"R"]
[]
[9,"Metal work",null,9,{"$nulls":3},"R"]
[]
[10,"Glazing",null,10,{"$nulls":3},"R"]
[]
[11,"Paint work",null,11,{"$nulls":3},"R"]
[]
[12,"Masonry",null,12,{"$nulls":3},"R"]
[]
[13,"Plastering",null,13,{"$nulls":3},"R"]
[]
[14,"Blinds",null,14,{"$nulls":3},"R"]
[]
[]
[null,"SUB TOTAL",{"$nulls":5},"R"]
[]
[null,"ADD VAT @ 15%",{"$nulls":5},"R"]
[]
[null,"TOTAL AMOUNT",{"$nulls":5},"R"]
{"$rows_empty":10}
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
[]
[null,"SECTION 3"]
[]
[null,"ELECTRICAL WORKS: SCHEDULE OF QUANTITIES"]
[]
[null,"PROVISIONAL SCHEDULE OF QUANTITIES "]
[]
[null,"Major Supply and Installation of Platform and Shelter Lighting at Lenz Station"]
[]
[null,"BILL NO. 1"]
[]
[null,"ALTERATIONS (PROVISIONAL)"]
[]
[null,"REMOVAL OF EXISTING WORK"]
[]
[null,"Taking out and removing electrical work"]
[]
[1,"400W HPS fittings",null,"No.",4]
[]
[2,"Bulkhead fittings",null,"No.",50]
[]
[3,"4/5 foot fluorescent fittings",null,"No.",35]
[]
[4,"High Bay 400w light fittings",null,"No.",15]
[]
[{"$nulls":4},"Carried to final summary"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
[]
[null,"BILL NO.2"]
[]
[null,"ELECTRICAL WORK"]
[]
[null,"Supply, install test commission and hand over"]
[null,"in good working conditions complete the"]
[null,"electrical system as per BoQ, specifications, IEE wiring regulations & as required by Local Electrical Authorities (NEC) for the complete project all up to the Satisfaction of the Engineer. All the material to be supplied to bear SABS mark or SABS mark of compliance."]
[]
[null,"Fluorescent fittings waterproofed fixture white including 2x58w T8 LED Fluorescent tubes and polycarbonate base with clear polycarbonate cover IP65"]
[]
[1,"Waterproof polycarbonate LED 5ft 2 x58w T8 fluorescent fitting including 2 LED tubes",null,"No.",20]
[]
[2,"1200m (4 foot) 2x36w Open channel cool white LED Fluorescent fittings double tubes for ticket office building",null,"No.",25]
[]
[null,"Bulkhead fittings"]
[]
[3,"Corrosion resistance high pressure die- cast aluminium  LED 19w Bulkhead fitting with wire guard IP 65 bearing the SABS Mark minimum 50 000hrs lifetime 4 000K at a colour rendering index >70, injection moulded high impact acrylic diffuser  including opening tool for platform shelters",null,"No.",35]
[]
[4,"7w LED bulk head  fittings completely with bulbs",null,"No.",15]
[]
[null,"HIGH BAY LED FITTINGS"]
[]
[null,"279W LED Lumminaire (34460 lumen) with 3 an optical compartment with LED engine, glass protector, LED warm light with colour temperature of 3000 kelvin, gear compartment and a spigot top entry adjustable compartment. Both optical and gear compartments to be rated IP 66. 20kV/kA surge protection. The luminaire housing to be manufactured of marine grade cast aluminium (EN 1706 AC-44300). Including 1 opening tool"]
[]
[null,"The use of cherry picker/scaffolder or any other equipment to be used for replacing of masts pole fittings and bulbs for the duration of the project"]
[]
[5,"389 x 389 x 168mm 203W LED Lumminaire 32260 lumen) compartment with LED engine, glass protector, LED neutral white 740 with colour temperature of 4000 kelvin, Both optical and gear compartments to be rated IP 66. 10kV/kA surge protection. The luminaire housing to be manufactured of Marine grade high pressure die cast aluminium (EN 1706 AC 44300) optical housing Eco bay fittings to bears the SANS 60598 safety mark",null,"No.",15]
[]
[null,"High mast pole street light fitting"]
[]
[6,"279W LED Lumminaire (34460 lumen) with 3 an optical compartment with LED engine, glass protector, LED warm light with colour temperature of 3000 kelvin, gear compartment and a spigot top entry adjustable compartment. Both optical and gear compartments to be rated IP 66. 20kV/kA surge protection. The luminaire housing to be manufactured of marine grade cast aluminium (EN 1706 AC-44300). Including 1 opening tool",null,"No.",4]
[]
[7,"835x 345 x 35cm 265W LED MAXI light Lumminaire 43584 lumen)  with LED engine, glass protector, LED warm light with 730 colour temperature of 3000 kelvin, gear compartment and a spigot top entry adjustable compartment. Both optical and gear compartments to be rated IP 66. 20kV/kA surge protection. The luminaire housing to be manufactured of marine grade cast aluminium (EN 1706 AC-44300). Including 1 opening tool",null,"No.",18]
[]
[null,"SWITCHES"]
[]
[8,"Day light switches  ",null,"No.",4]
[]
[9,"11 kw contactors",null,"No.",3]
[]
[10,"White 1 lever 2 way switch",null,"No.",15]
[]
[11,"White 2 lever 1 way switch",null,"No.",6]
[]
[null,"Electrical cables"]
[]
[12,"70mm2 4 core armored cable in trenches measured else where  ",null,"m",250]
[]
[13,"25mm2 4 core armored cable in trenches measured else where  ",null,"m",450]
[]
[14,"16mm2 4 core armored cable in trenches measured else where  ",null,"m",100]
[]
[15,"10mm2 4 core armored cable in trenches measured else where  ",null,"m",400]
[]
[16,"4mm2 4 core armored cable in trenches measured else where  ",null,"m",100]
[]
[17,"2.5mm2  GP wires (Red, white, blue, black and earth) for lights rewiring of  shelters in 3 phase system",null,"m",100]
[]
[18,"2.5mm2 suffix cable or GP wire ",null,"m",200]
[]
[19,"1.5mm2 suffix cable or GP wire for lights",null,"m",200]
[]
[null,"Electrical casing"]
[]
[20,"20mm galvanized SABS conduit completely with all the couplings, galvanized saddle, spacer bar assembly and heavy duty U clamps completely encased 100mm deep on concrete walls and make good  ",null,"m",150]
[]
[21,"20mm PVC SABS conduit completely with all the couplings, saddle, spacer bar assembly and heavy duty U clamps",null,"m",100]
[]
[22,"40 x 25mm white heavy duty PVC trunking comlpetely with all the fittings",null,"m",50]
[]
[23,"76 x 76 X 0.8 mm galvanized  heavy duty steel trunking comlpetely with all the fittings",null,"m",30]
[]
[null,"PLUGS"]
[]
[24,"4 x 4 Double plug",null,"No.",10]
[]
[25,"4 x 4 single plug",null,"No.",10]
[]
[null,"Circuit breakers "]
[]
[26,"10 A 1P 6KA single circuit breaker",null,"No.",20]
[]
[27,"10 A 3P 6KA circuit breaker",null,"No.",5]
[]
[28,"12 A 3P Contactor",null,"No.",2]
[]
[29,"20 A 1P 6KA single circuit breaker",null,"No.",25]
[]
[30,"20 A 3P 6KA circuit breaker",null,"No.",3]
[]
[31,"30 A 1P 6KA circuit breaker",null,"No.",3]
[]
[32,"30 A 2P 6KA circuit breaker",null,"No.",3]
[]
[33,"40 A 2P 6KA circuit breaker",null,"No.",3]
[]
[34,"60 A 3P AC1 Contactor",null,"No.",2]
[]
[35,"63 A 2P 6KA circuit breaker",null,"No.",2]
[]
[36,"63 A 3P 6KA circuit breaker",null,"No.",2]
[]
[37,"63 A 30Ma 3P + N Earth leakage",null,"No.",2]
[]
[38,"400 A 3P Main circuit breaker",null,"No.",1]
[]
[39,"250 A 3P Main circuit breaker",null,"No.",2]
[]
[40,"80 A 3P Main circuit breaker",null,"No.",1]
[]
[41,"60 A 3P Main circuit breaker",null,"No.",1]
[]
[42,"60 A 4 x 4 2 pole stove Isolator",null,"No.",1]
[]
[43,"30A Air conditioner  Isolator",null,"No.",2]
[]
[null,"DB BOARDS"]
[]
[44,"Surface mounted  min distribution board for staffroom (4 offices, one kitchen and 2 separate toilets )completely with circuit breakers",null,"No.",3]
[]
[45,"1000h x 400w x 400d x 2.0mm stainless steel orange IP 65 weatherproofed floor mounted lockable Station kiosk with 1 door completely rewired with all the circuit breakers mounted on din rail as per above and all other accessories, connected to the station",null,"No.",1]
[]
[46,"Lockable fiber glass water proofed 12 way CBI DB  Eaves box to be mounted on external walls for platform shelters, waiting areas, access point, ablutions, etc",null,"No.",10]
[]
[null,"HVAC Systems"]
[]
[47,"Supply, install and commission new 24000 BTU split unit, inverter technology air conditioner completely with all accessories (drain pipe, amorflex, copper pipe, refrigerant, cable, communication wire, brackets, circuit breaker, isolator, etc )",null,"No.",3]
[]
[null,"PLATFORM/STREET HIGH MAST STEEL POLES"]
[]
[null,"Pricing shall includes the design, supply, delivery to site, off-loading, erection, installation, commissioning, testing, and handing over in full working order a high mast lighting structure, including floodlight luminaries."]
[]
[null," The works specifically include the following: "]
[]
[null,"1. Geotechnical studies of proposed sites and issuing of soil test results. "]
[]
[null,"2. Design, preparation and cast of appropriate foundations. "]
[]
[null,"3. Design, supply, delivery to site, off-loading, erection, installation, commissioning, testing, and handing over in full working order a 30 meter high mast pole complete with Luminaries and control panel as specified."]
[]
[null,"4. Perform an electrical connection to the installation from the station kiosk"]
[]
[null,"5. Test and commissioning of the high mast lighting installation. "]
[]
[null,"6. Issuing of a certificate of compliance (COC) in terms of SANS 0142 Code of Practice.  "]
[]
[null,"7. all works should be accordance with the relevant specified specification (wirireing code SANS 0225)"]
[]
[null,"8. 30m high mast light shall be operated and maintaned in the horizontal position by means of a mechanical a mechanical winch "]
[]
[null," Tests "]
[]
[48,"Soil geotechnical studies for foundation including soil and concrete cube tests. ",null,"Per Pole",2]
[]
[49,"Perform soil bearing pressure tests for each mast prior to casting the concrete base to ensure that the soil load bearing conditions are suited to the specific concrete base design. Provide soil test Certificate ",null,"Per Pole",2]
[]
[50,"Test earth system and provide test certificate ",null,"Per Pole",2]
[]
[null,"Earth works"]
[]
[51,"Concrete foundation for high mast complete as per manufactrures specifications with excavation not exceeding 2m deep, steel reinforcing, cables inlet pipes, earth spikes, foundation bolts and template set, back fill material and soil concrete test.",null,"Per Pole",2]
[]
[null,"The use of Crane during the installation of 30m high mast poles"]
[]
[52,"Supply and deliver to site 30m above the ground HDG galvanized street pole with 9way Spiggot to recieve 9 lights per pole, LED Street lights priced elsewhere. Assemble and Erect complete with all accessories, distribution board, internal cables, carriage, earthing with 2 x earth spikesetc.  ",null,"No.",2]
[]
[null,"DOUBLE DRUM WORM WINCH "]
[]
[null,"H:328 MM, W:410mm, M:80kg "]
[]
[null,"Dymot DD800W Double drum Worm Winch "]
[]
[null,"S.W.L.: 800kg   (400kg +400kg) "]
[]
[null,"Rope DIA:6mm "]
[]
[null,"Drum Rope Capacity: 33m "]
[]
[null,"Gear Ratio:  50:1 "]
[]
[null,"Handle Radius:   285 "]
[]
[null,"Swive Base "]
[]
[null,"dia (7x19) Stainless Steel Rope Sling,  33 long "]
[]
[null,"C/W Stainless Thimble & Copper Ferule one end only. "]
[]
[null,"Power Tool "]
[]
[null,"220V Electric Power Tool "]
[]
[null,"c/w Torgue limiter & 3m remote cable "]
[]
[53,"Double Drum Worm Winch completely including, remote, Swive Base, power tools etc used for for lowered of high mast poles ",null,"No.",1]
[]
[null,"SLEEVE"]
[]
[54,"110mm HDPE double wall corrugated coil with 5mm plain galvanized draw wire per sleeve. Both ends to be plugged before backfilling",null,"m",900]
[]
[null,"EARTHING"]
[]
[55,"Earth bonding (water pipes, stoves, etc)for the whole station as per SANS 10142 and"]
[null,"the specification.",null,"Item",1]
[]
[null,"ELECTRICAL COMPLIANCE"]
[]
[null,"All work to comply to SANS 10142"]
[null,"Compliance certificate to be provided on completion"]
[null,"Pricing to include all necessary complete connection"]
[]
[56,"Certificate of compliance and all other testing required including 12 month guarantee certificate",null,"Item",1]
[]
[{"$nulls":4},"Carried to final summary"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
[]
[null,"BILL NO. 3"]
[]
[null,"EARTHWORKS"]
[]
[null,"EXCAVATION, FILLING, ETC"]
[]
[1,"Removing and relaying of paving blocks after cables has been laid. To be relayed as per manufactures specification",null,"m²",750]
[]
[2,"220 x 108.5 x 50mm, classification:PA, 40.0 brick strength with 7.4% water absorption layed as per manufactures specification",null,"m²",100]
[]
[null,"Excavation in earth not exceeding 2m deep"]
[]
[null,"Trenches"]
[]
[null,"Earth filing obtain from the excavation and/or prescribed stock piles on site compacted to 90% Mod AASHTO density"]
[]
[3,"Backfilling to holes after concrete has been laid ",null,"m3",700]
[]
[null,"15 Mpa/20 mm unreinforced concrete"]
[]
[4,"1m long * 0.5m wide  x 0.2m thick Concrete block on every five meter interval on top of 16 mm² 4-core underground cable",null,"m3",20]
[]
[{"$nulls":4},"Carried to final summary"]
[]
[]
[]
[]
[]
[]
[null,"FINAL SUMMARY "]
[null,"ELECTRICAL WORK AT LENZSTATION"]
[]
[]
[null,"SECTION No.3"]
[]
[1,"ALTERATIONS",null,"BILL No.1",{"$nulls":3},"R"]
[]
[2,"ELECTRICAL WORK",null,"BILL No.2",{"$nulls":3},"R"]
[]
[3,"EARTHWORKS ",null,"BILL No.3",{"$nulls":3},"R"]
[]
[]
[]
[null,"SUB TOTAL",{"$nulls":5},"R"]
[]
[null,"ADD VAT @ 15%",{"$nulls":5},"R"]
[]
[null,"TOTAL AMOUNT",{"$nulls":5},"R"]
[]
[]
[]
[]
[]
[]
[null,"FINAL SUMMARY "]
[null,"MINOR WORKS AT LENZ STATION"]
[]
[]
[]
[]
[1,"PRELIMINARY AND GENERAL ",null,"SECTION No.1",{"$nulls":3},"R"]
[]
[2,"CIVIL AND GENERAL BUILDING WORK AT LENZ STATION",null,"SECTION No.2",{"$nulls":3},"R"]
[]
[3,"ELECTRICAL WORK",null,"SECTION No.3",{"$nulls":3},"R"]
[]
[]
[]
[]
[null,"SUB TOTAL",{"$nulls":5},"R"]
[]
[null,"ADD VAT @ 15%",{"$nulls":5},"R"]
[]
[null,"TOTAL TENDER AMOUNT",{"$nulls":5},"R"]

{"sheet":"MIDWAY","index":2,"n_rows":1220,"n_cols":8,"rows_kept":1220,"merged":[[0,0,0,1],[5,0,5,1],[30,4,30,6],[144,3,144,5],[173,3,173,5],[198,3,198,5],[226,3,226,5],[302,4,302,6],[350,4,350,6],[413,4,413,6],[619,4,619,6],[654,4,654,6],[686,4,686,6],[758,4,758,6],[780,4,780,6],[816,4,816,6],[828,4,828,6],[870,1,870,5],[872,1,872,5],[874,1,874,5],[910,4,910,6],[1138,4,1138,6],[1166,4,1166,6],[1189,1,1189,5],[1191,1,1191,5],[1193,1,1193,5],[1215,1,1215,5],[1217,1,1217,5],[1219,1,1219,5]],"flags":["formulas_cached_only"]}
[]
[]
[null,"SCHEDULE OF QUANTITIES "]
[]
[null,"MINOR UPGRADES AT MIDWAY STATION: RFQ NO:13/07/2022/06CRES"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
["No"]
[null,"SECTION 1"]
[]
[null,"BILL NO. 1"]
[]
[null,"PRELIMINARY AND GENERAL "]
[]
[null,"Preliminary and General"]
[]
[1,"All Preliminary and General applicable to this project",null,"Sum",1]
[]
[null,"Occupational Health and safety"]
[]
[null,"The contractor shall comply with all the requirements set out in the Construction Regulations, issued under The Occupational Health & Safety Act no 85 of 1993."]
[]
[null,"Safety file shall be provided by the contractor prior to commencement of work."]
[]
[null,"The contractor shall carry out the works with as little noise and mess as possible. All rubble shall be taken away from site on a daily basis."]
[]
[null,"Note: All designated items should comply with local content threshold. "]
[]
[2,"Compliance with Occupational Health and Safety Act (Act 85 of 1993) and its regulations and with the Employers Health and Safety",null,"Sum",1]
[]
[{"$nulls":4},"Carried to final summary"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
["No."]
[null,"SECTION NO. 2"]
[]
[null,"CIVIL AND GENERAL BUILDING WORK AT MIDWAY STATION"]
[]
[null,"BILL NO. 1 "]
[]
[null,"ALTERATIONS  "]
[]
[null,"SUPPLEMENTARY PREAMBLES  "]
[]
[null,"General "]
[]
[null,"Special care shall be exercised during the progress of the"]
[null," work to ensure that any electrical installations, water supply"]
[null," pipes, telephone and other services which may be"]
[null," encountered are not interfered with and notice shall be given"]
[null," to the project manager if any disconnection or"]
[null," alterations become necessary"]
[]
[null,"The contractor shall take all precautions necessary to"]
[null," prevent any nuisance from dust whilst carrying out the work"]
[]
[null,"Leave in good condition"]
[]
[null,"The contractor must leave the existing building,in which "]
[null,"the alterations are executed ,clean and neat at completion"]
[]
[null,"Price shall include removal and disposal of rubble from site"]
[]
[null,"REMOVAL OF EXISTING WORK  "]
[]
[]
[null,"Taking down and removing ceiling"]
[]
[1,"Suspended ceiling",null,"m²",50]
[]
[2,"Rhino Board ",null,"m²",150]
[]
[null,"Taking down and removing doors"]
[]
[3,"Timber single door 813 x 2032",null,"No.",10]
[]
[null,"Taking out and removing glass, beads, etc"]
[]
[4,"Brocken window pane from steel frame including upgrading, cleaning and preparation to receive new",null,"m²",15]
[]
[null,"Hacking up/off and removing ceramic tile floor and wall finishes including removing mortar bed or backing and preparing concrete or brick surface for new screed, plaster or tile finishes"]
[]
[5,"150 x 150mm tiles to walls",null,"m²",50]
[]
[6,"300 x 300mm tiles to floors",null,"m²",50]
[]
[null,"Taking out and removing piping, sanitary fittings, etc including disconnection piping from fittings"]
[]
[7,"9l Ceramic pan and cistern ",null,"m²",15]
[]
[8,"wash hand basin including all fittings",null,"No",7]
[]
[9,"Down pipes",null,"m",50]
[]
[10,"Gutters",null,"m",100]
[]
[null,"Taking out and removing"]
[]
[11,"2000 x 2000mm high blinds",null,"No",15]
[]
[null,"SERVICING, REPAIRING, RE-FIXING, CLEANING, ETC OF EXISTING WORK",null,"No",4]
[]
[null,"Clean down existing roof sheeting, box gutters, flashings. Etc apply de-rusting compound to surfaces, prepare area for paint application and allow for re-fixing, replacing and waterproofing of necessary roof screws, fixing screws, etc"]
[]
[12,"IBR roof sheeting in fair condition not exceeding 30 degree slope",null,"m²",100]
[]
[13,"Sheet steel box gutters in fair condition",null,"m",200]
[]
[null,"Re-fixing and aligning of fascia and barge boards"]
[]
[14,"Fibre cement fascia and barge boards not exceeding 300mm girth",null,"m",50]
[]
[15,"Sheet metal fascia and barge boards not exceeding 300mm girth",null,"m",50]
[]
[null,"Clean down existing facebrick façade, painted walls, plinths, wall tiles, floor tiles, etc with water and brush "]
[]
[16,"Internal and external face brick walls",null,"m²",500]
[]
[17,"Internal ceramic wall and floor tiles",null,"m²",200]
[]
[null,"Clean down existing window panes"]
[]
[18,"Glazing to steel windows measured on both sides",null,"m²",100]
[]
[null,"Clean out and service gutters"]
[]
[19,"125 x 100mm eaves gutter",null,"m",100]
[]
[20,"250 x 200mm industrial eaves gutter",null,"m",100]
[]
[null,"Upgrading of stormwater and Sewer network"]
[]
[21,"High pressure jetting and cleaning of 300mm diameter stormwater underground pipe",null,"m",350]
[]
[22,"High pressure jetting and cleaning of 110mm diameter sewer underground pipe",null,"m",350]
[]
[null,"Servicing existing steel industrial Roll-shutter doors including operating mecanism"]
[]
[23,"Roll up door size 4000 x 3000mm heigh",null,"No.",6]
[]
[null,"Taking out and removing boundary steel gate"]
[]
[24,"3000mm long x 2400mm high steel gate to be delivered at New Canada depot",null,"No.",3]
[]
[{"$nulls":3},"Carried to final summary"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
[]
[null,"BILL NO 2"]
[]
[null,"Earthworks (Provisional)"]
[]
[null,"Supplementary Preambles"]
[]
[null,"All soil poisoning and insecticide to be applied under a ten year guarantee by an approved firm of specialist"]
[]
[null,"General notes"]
[]
[null,"Fill material shall be placed in lift of not more than 150mm"]
[null,"Compaction density to be controlled using DCP apparatus to a maximum of 30mm/blow 93% MOD AASHTO compaction is to be achieved "]
[]
[null,"Where backfill is required on both sides of walls, backfill both sides simultaneously."]
[]
[null,"Where compaction of fill material behind retaining walls is done using mechanical rollers, the rollers must be kept 500mm away from the wall and this 500mm portion must be compacted with hand stampers or wackers."]
[]
[null,"Site Clearance"]
[]
[1,"Cleaning and removal of rubble from site",null,"m²",10000]
[]
[null,"G5 Material  compacted to 93% Mod AASHTO density"]
[]
[2,"Backfilling to trenches",null,"m",300]
[]
[{"$nulls":3},"Carried to final summary"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
[]
[null,"BILL NO 3"]
[]
[null,"CONCRETE WORK"]
[]
[null,"Application: Outdoor Litter Bin"]
[null,"External size: 700mm x 700mm x 875mm high"]
[null,"Internal size: 600mm x 600mm x 700mm deep"]
[null,"Capacity: 320 litres"]
[null,"Mass: 430kg"]
[null,"Finish: Exposed aggregate"]
[null,"Advertising space: 4 x 685mm x 590mm"]
[null,"Drainage hole in bottom"]
[]
[1,"Supply and deliver Advertising Bin with exposed aggregate external finish ",null,"No.",15]
[]
[null,"STEEL BRIDGE TREADS"]
[]
[null,"Reinforced Precast Concrete Bridge Treads"]
[]
[2,"2500mm long x 300mm wide x 80mm deep precast concrete bridge treads as per attached drawing with bending schedule",null,"No.",6]
[]
[{"$nulls":3},"Carried to final summary"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
[]
[null,"BILL NO 4"]
[]
[null,"ROOF COVERING ETC"]
[]
[null,"PROFILE METAL SHEETING AND ACCESSORIES"]
[]
[null,"Roof sheeting to be Concealed Fix interlocking \"KLIP-LOK 700\",  0,58mm thick heavy industrial Z275 spelter galvanised steel sheeting with Chromadek, ColorPlus, Colourbond or Globalcoat finish to one side and Grey other side and accessories, fixed to steel purlins using SL 700  approved clips and fasteners. Cover width 700mm. High wind - 120km/h plus - loading to be considered with installation and fixing must be in accordance with manufacturer's recommendations and specifications."]
[]
[1,"Roof covering with pitch not exceeding 25 degrees",null,"m²",20]
[]
[2,"450mm galvanized steel roll top ridge",null,"m",20]
[]
[null,"REPAIRS TO GALVANISED IRON ROOF COVERING"]
[]
[null,"Carfully examine entire roof area and locate leaks with particular attention"]
[null,"given to roof leaks where marks are available on walls and ceiling.Locate holes"]
[null,"and solder.Replace defective screws using longer screws as ''Reaseal'' or similar"]
[null,"approved as SABS Specification 135 where purlins are fixed on edge,and 6mm "]
[null,"bolts where purlins are fixed on flat.Beat into corrugation damaged or buckled"]
[null,"edges,fix in position where necessary using self tapping screws,roofing screws"]
[null,"or verandah bolts.Similarly examine all flashing,ridging and vally linings,"]
[null,"repair and refix loose sections,as for the roof covering.No plastic or other"]
[3,"compounds are to be used to render leaks watertight.",null,"m²",2000]
[]
[{"$nulls":3},"Carried to final summary"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
[]
[null,"BILL NO. 5"]
[]
[null,"CARPENTRY AND JOINERY  "]
[]
[null,"TIMBER  "]
[]
[null,"All softwood to be South African Pine  "]
[]
[null,"DOORS, ETC"]
[]
[null,"Wrought meranti doors hung to steel frames"]
[]
[null,"44mm thick exterior grade flush solid core timber single door with 3mm thick commercial ply on both sides with consolidated edges fitted and complying with SABS 545 in pressed steel frame. All painted in accordance with architect's colour schedules"]
[]
[1,"813 x 2032 x 44mm single leaf solid core with commercial veneer for paint. pricing shall include painting as per manufactures specification",null,"No.",10]
[]
[2,"1500 x 2032 x 44mm single leaf solid core with commercial veneer for paint. pricing shall include painting as per manufactures specification",null,"No.",1]
[]
[null,"44mm thick interior grade flush solid core timber single door with 3mm thick commercial ply on both sides with consolidated edges fitted and complying with SABS 545 in pressed steel frame. All painted in accordance with architect's colour schedules"]
[]
[3,"813 x 2032 x 44mm single leaf solid core with commercial veneer for paint. pricing shall include painting as per manufactures specification",null,"No.",15]
[]
[null,"FITTINGS"]
[]
[null,"The following in modular timber cupboards, counters, duty stations, desk etc. as per Cupboard Connections Specification"]
[]
[null,"Carcasses of 16mm thick particle board with both faces white melamine with white Masonite backs. Shelving of 16mm particle board, both faces white melamine and front edge in white PVC. Doors of 16mm particle board with post formed vertical edges and laminated in Renolit. Tops of 32mm particle board with post formed leading edges and laminated in high pressure decorative laminate. All butt edges and edges against walls to be sealed with silicon sealant. Hinges to be “Hettich”. Drawer runners to be metal 500mm series with nylon runners or similar. All units complete with door, handles, hinges, cupboards, door, locks, barrel bolts and shelves. Floor unit complete with kick plates. (Formica tops measured elsewhere)   "]
[]
[null,"Built in cupboards fittings"]
[]
[null,"General"]
[]
[null,"The following cupboard fittings have been measured as complete units i.e. the components of the units have not been separately measured. The descriptions, therefore, of such units shall be deemed to include all components, assembling, housing, notching, glueing, blocking, planting on and screwing with countersunk screws, edge strips, decorative plastic finish, glass, ironmongery, metalwork and paint or varnish finishes"]
[]
[null,"Ticket sales work stations"]
[]
[4,"1000H x 700W x 700mmD Floor cupboard with lockable shelf / drawer and single hinged door to match Pollak Park Ticket Office counter (Top measured elsewhere)",null,"No.",3]
[]
[null,"Kitchen cupboards,etc."]
[]
[5,"Kitchen sink floor cupboard 2000 x 600 x 900mm high with sides, bottom, back, 3 hinged doors and one drawer completely working including handles, etc. top and sink measured else where",null,"No.",2]
[]
[null,"Interior type particle board with Formica veneer "]
[]
[6,"900 x30mm thick granite with all exposed edges large bevel edged, fixed to supports using dabs of 100% black silicone adhesive along all supports with all joints filled with matching polyester resin glue. Granite surface to be sealed using an approved stone sealer, all in accordance with the manufacturer's recommendations.",null,"m",15]
[]
[7,"2mm thick edge strip 32mm wide",null,"m",10]
[]
[8,"Cut 50mm work top to fit end bowl sink, measured else where ",null,"No.",4]
[]
[null,"EAVES, VERGES, ETC"]
[]
[null,"Pressed fibre cement"]
[]
[9,"10 x 225mm Fascia’s including galvanized steel H-Profile jointing strips",null,"m",60]
[]
[10,"10 x 230mm Barge boards including galvanized steel H-profile jointing strips ",null,"m",25]
[]
[null,"Wrought softwood "]
[]
[11,"50 x 75mm purlins at 900mm center’s to sides of trusses ",null,"m",60]
[]
[12,"38mm x 114mm wall plates ",null,"m",30]
[]
[13,"38mm x 100mm Grade M4 ridge beam",null,"m",30]
[]
[14,"50mm x 75mm purlins",null,"m",60]
[]
[null,"Sundries"]
[]
[15,"Two coats creosote on sawn timbers",null,"m²",80]
[]
[{"$nulls":4},"Carried to final summary"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
[]
[null,"BILL NO 6"]
[]
[null,"CEILING WORK"]
[]
[null,"SUPPLEMENTARY PREAMBLES "]
[]
[null,"Description "]
[]
[null,"Items described as “nailed” shall be deemed to be fixed with hardened steel nails or pins or shot pinned to brickwork or concrete"]
[]
[null,"Items described as “plugged” shall be deemed to include screwing to fibre, plastic or metal plugs at not exceeding 600mm centres, and where described as “bolted”, bolts priced elsewhere"]
[]
[null,"Finishes to suspended ceilings:"]
[]
[null,"All finishes to be applied at the factory during the manufacturing process and to be delivered on site “pre-finished” as described. No applying of finishes on site will be allowed"]
[]
[null,"NAILED UP CEILING"]
[]
[null,"6mm “Everite Nutec” fibre cement boards with H-type pressed steel jointing including painting with one coat of alkali resistance primer , one undercoat and two coat eggshell enamel paint"]
[]
[1,"Ceiling generally 600mm wide including 38 x 38mm sawn softwood brandering at maximum 600mm centres nailed to and including 75 x 50mm sawn softwood bearers at 900mm centres suspended approximately 250mm below timber trusses with 75 x 38mm vertical bearers at 600mm centres nailed to tie beams of trusses",null,"m²",150]
[]
[2,"Extra over ceiling for 800 x 800mm trap door of 38 50mm wrought softwood rebated framing with one 38 x 38mm sawn softwood cross brander covered with ceiling board and fitted flush in opening",null,"No.",3]
[]
[null,"“Rhino” gypsum plasterboard cornice"]
[]
[3,"75mm coved cornices fixed to ceiling",null,"m",200]
[]
[null,"SUSPENDED CEILING"]
[]
[null,"OWAcoustic(R) Futura Premium biologically absorbable mineral wool ceiling tiles, NRC - 0.75, size 1200 x 600 x 15mm with Square-edge and white painted finish, laid on fire rated OWAconstruct(R) system S3 exposed demountable  T24 suspension system, comprising galvanised main tees and cross tees with main tees suspended by means of galvanised hangers at centres not exceeding 1200mm with ceiling perimeter finished with OWAconstruct Shadowline W-trim, plugged and screwed at 200mm centres, and all installed to manufacturer's instructions."]
[]
[4,"Suspended ceiling not exceeding 1m below concrete soffit",null,"m²",25]
[]
[null,"Cornices to suspended ceiling"]
[]
[5,"Standard brilliant white pre-painted metal angle cornices plugged",null,"m",50]
[]
[null," Perforated lay-in powder coated aluminium ceiling tiles"]
[]
[null,"Lay-In system comprising 600 x 600 x 0,6mm thick aluminium acoustic tiles finish colour RAL 9010 with 8mm reveals and 1,5mm diameter perforations including sound absorbing non woven tissue backing, laid on T15 suspension system including main tees at 1200mm centres, cross tees, etc. all suspended with galvanised hangers at not exceeding 1200mm centres. Ceiling perimeter finished with W-profile. The whole to be designed and installed by approved specialist, all in accordance with the manufacturer's recommendations."]
[]
[6,"Suspended ceiling not exceeding 1m below concrete soffit",null,"m²",30]
[]
[{"$nulls":4},"Carried to final summary"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
[]
[null,"BILL NO 7"]
[]
[null,"IRONMONGERY"]
[]
[null,"LOCKS"]
[]
[null,"Supply and install"]
[]
[1,"Ultra-security heavy duty double pin locks",null,"No",10]
[]
[2,"3 liver mortice lockset with handles",null,"No",30]
[]
[3,"Indicator door lock chrome plated",null,"No",15]
[]
[4,"90mm square Padlock",null,"No",4]
[]
[5,"6 pin tumbler key system, mortice dead lock with an additional heavy duty magnetic lock and striker including key switch for bullet proof door",null,"No",1]
[]
[null,"BATHROOM FITTINGS  "]
[]
[6,"Satin stainless-steel toilet roll holders for 2 rolls with central shaft system and cylinder lock, plugged and screwed to the wall with stainless steel screws. (vandal resistant)",null,"No",4]
[null," "]
[null,"Door closer"]
[]
[7,"Heavy duty slide arm door closer",null,"No",5]
[]
[null,"SIGNAGE"]
[]
[null,"External signage"]
[]
[null,"Male Signage"]
[]
[8,"500 x 500 x 3mm mild steel ACM panel with vinyl graphic overlay",null,"No",1]
[]
[null,"Female Signage"]
[]
[9,"500 x 500 x 3mm mild steel ACM panel with vinyl graphic overlay",null,"No",1]
[]
[null,"Paraplegic Signage"]
[]
[10,"500 x 500 x 3mm mild steel ACM panel with vinyl graphic overlay",null,"No",1]
[]
[null,"Double Sided Platform Station Name "]
[]
[11,"2100mm x 3000 x 3mm mild steel ACM panel sprayed to Pantone 3005C with vinyl graphic overlay and white vinyl graphics mounted on 65mm diameter x 2.6m high above the ground mild steel poles in concrete footing ",null,"No",3]
[]
[null,"Stainless Steel Grade 304 Platform Public Seating"]
[]
[null,"Arms and Legs: Aluminium Die-Cat, chromed. "]
[]
[null,"Cross beam: 2mm Aluminium extrusion, silver. "]
[]
[null,"Seat and back: Stainless steel "]
[]
[12,"5 Seater 2890mmW x 670mmD x 785mmH Peforated Aluminium chairs suitable for outdoors burried on earth less then 1mm deep including excavation, concrete, backfilling, etc",null,"No",10]
[]
[null,"ALUMINIUM WINDOWS "]
[]
[13,"Window type HS1812 Bronze Powder coated 1800 x 1200mm high aluminum sliding window",null,"No",1]
[{"$nulls":4},"Carried to final summary"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
[]
[null,"BILL NO 8"]
[]
[null,"PLUMBING WORK "]
[]
[null,"SANITARY FITTINGS"]
[]
[1,"Vandal resistance low level High traffic suite complete (Front flush), suite to includes CC  white Cistern made from high strength technoplast polymer with concealed mounting bracket, heavy duty securing bolts, concealed tamper proof lid screws and hiflo MK3 flush valve, including CC Pan and and heavy duty seat.",null,"No",5]
[]
[2,"Concealed Anti-vandal high traffic suite (Front flush), CC Cistern excluding CC Pan",null,"No",5]
[]
[3,"Paraplegic vitreous china floor mounted paraplegic washdown suite colour White (Code: 7300SC) comprising semi close couple 90º outlet open rim washdown pan and matching 9 litre cistern, including lid, fitments and purpose-made chromium plated side flush lever.\n",null,"No",1]
[]
[4,"Close coupled suite colour White , comprising 90º outlet open rim pan with matching 9 litre front single flush cistern including lid and fitments and Jazz Thermoset seat.",null,"No",7]
[]
[5,"Ceramic wash hand basin colour White, size 510 x 405mm with one tap hole including integrated overflow and chain stay hole bolted to wall with two x 10mm bolts and including Classic floor mounted pedestal and sealed with silicone sealant where basin meets wall.",null,"No",10]
[]
[6,"China drop-in vanity basin colour White (Code: 7034), size 420 x 420mm fitted into opening in granite vanity top (elsewhere specified) and sealed with silicone sealant where basin rim meets vanity top.  To be used in conjunction with wall mounted push on demand tap as specified V05-V06.",null,"No",6]
[]
[]
[null,"URINAL BASIN"]
[]
[7,"Sanitary ware white vitreous wall mounted urinal with top inlet or back inlet . Overall size 600x385x380mm. Supplied with 38mm c.p. domical grating, a spreader(with a 20mm tread) and two hanger brackets",null,"No",3]
[]
[8,"1830 x 1220mm high floor mounted curved manual flush urinal Centre outlet manufactured from stainless steel AISI 304 including 20Mpa/20mm for installation and unreinforced concrete slab",null,"No",2]
[]
[null,"SINK, BASIN, ETC"]
[]
[9,"Grade 430 stainless steel double bowl sink and drainer size 1160 x 460mm with tiling key, 40mm chromium plated flanged outlets and waste unions, vulcanite or rubber plugs, chromium plated chains and stays, 40mm rubber resealing P-trap with extension piece and clamped connections",null,"No.",2]
[]
[null,"TAPS, VALVES, ETC"]
[]
[null,"Supply and install"]
[]
[10,"Self-closing push button tap",null,"No.",10]
[]
[11,"15mm chrome plated deck mounted sink mixer with overarm swivel outlet and adjustable flanges, manufactured in accordance with SANS 226:2004 Type 1.",null,"No.",2]
[]
[12,"Medical elbow action pillar tap with raised nose or equal approved, chrome finish. SANS 226 TYPE 2. ",null,"No.",1]
[]
[13,"15mm brass garden  tap ",null,"No.",2]
[]
[14,"Exposed type urinal flush valve with ball-o-stop, wall flange, chrome plate finish and non-hold open feature",null,"No.",3]
[]
[15,"15mm Ø BSP built-in sleeve, DZR brass urinal flush valve with internal flow control, strainer and no-hold feature for single bowl urinal.",null,"No.",2]
[]
[16,"Flexi connector",null,"No",30]
[]
[17,"15 Brass Gate Valve ",null,"No",4]
[]
[18,"Mini Ball Valve ",null,"No",30]
[]
[19,"22mm Brass Gate Valve including cast iron valve box",null,"No",2]
[]
[null,"WASTE UNINON ETC"]
[]
[20,"Basin waste, plug, chain, stay and backnut  ",null,"No.",10]
[]
[null,"TRAPS ETC"]
[]
[21,"38mm sink “P” trap",null,"No.",10]
[]
[22,"365/40 CP bottle trap 40 x 40 INC CP/PVC adaptor to 40mm suitable for wash hand basin and urinal ceramic basin",null,"No.",5]
[]
[23,"110mm pan connector completely ",null,"No.",14]
[]
[null,"WATER SUPPLIERS"]
[]
[null,"Class “O” copper pipe "]
[]
[24,"15mm pipes ",null,"m",20]
[]
[25,"15mm pipes chased into brick walls and make good",null,"m",35]
[]
[26,"22mm pipes ",null,"m",10]
[]
[27,"22mm pipes chased into brick walls",null,"m",10]
[]
[28,"Extra over class “O” copper pipes for capillary fittings"]
[]
[29,"15mm fitting  ",null,"No.",10]
[]
[30,"22mm fitting  ",null,"No.",5]
[]
[31,"15mm Tee",null,"No.",10]
[]
[32,"22mm Tee",null,"No.",5]
[]
[null,"Galvanized pipe "]
[]
[33,"32mm pipes ",null,"m",10]
[]
[null,"Extra over class Galvanized pipes for capillary fittings"]
[]
[34,"32mm fitting  ",null,"No.",3]
[]
[35,"32mm elbow  ",null,"No.",2]
[]
[36,"32mm Tee",null,"No.",2]
[]
[null,"Plastic pipe"]
[]
[37,"75mm high pressure plastic pipes in trenches less than 2m deep",null,"m",50]
[]
[38,"75mm gate valve",null,"No.",1]
[]
[39,"Male adaptor",null,"No.",6]
[]
[40,"Straight coupling",null,"No.",6]
[]
[null,"Plastic waste pipes"]
[]
[41,"50mm waste pipes with all connection and make good",null,"m",50]
[]
[null,"SOIL DRAINAGE"]
[]
[null,"Upvc class 34 pipes including excavation, bedding, backfilling and compaction and disposal of surplus material"]
[]
[42,"110mm pipes laid in and including trenches not exceeding 1m deep",null,"m",50]
[]
[43,"Extra over Upvc class 34 pipes for fittings",null,"No.",6]
[]
[44,"110 Bend",null,"No.",5]
[]
[45,"110mm junction",null,"No.",4]
[]
[46,"110mm Access bend",null,"No.",2]
[]
[null,"Sundries"]
[]
[47,"110mm Upvc cleaning eye to end of 110 Upvc pipe",null,"No.",2]
[]
[48,"350 x 350 x 50mm thick precast concrete inspection eye marker slab finished smooth on exposed surfaces with letters “I.E” or “I.O” on top and placed flush in ground or paving",null,"No.",2]
[]
[49,"Testing soil drainage system ",null,"Item",1]
[]
[null,"WATER RETICULATION"]
[]
[null,"PREAMBLES"]
[]
[null,"The contractor is referred to the General Preambles for trades 2017 published by the Association of South Africa Quantity Surveyors before pricing"]
[]
[null,"WATER PIPEWORK"]
[]
[null,"HDPE PE 100PN 12.5 pipes including excavation, bedding, backfilling, and compaction and disposal of surplus material"]
[]
[null,"High density polyethylene class 16 pipes"]
[]
[50,"25mm pipes with all other required connections laid in and including trenches ",null,"m",100]
[]
[51,"25mm fitting  ",null,"No.",3]
[]
[52,"25mm elbow  ",null,"No.",2]
[]
[53,"25mm Tee",null,"No.",2]
[]
[54,"Testing water supply system ",null,"Item",1]
[]
[null,"PLATFORM MANHOLE COVERS AND FRAMES"]
[]
[]
[55,"Type 9B MD polymer lid and frame including to make good after completion",null,"No.",10]
[]
[56,"600 x 900mm polymer lid and frame including to make good after completion",null,"No.",15]
[]
[null,"ELECTRIC WATER HEATERS"]
[]
[null,"Supply, deliver and install Electrical geysers with all other accessories  "]
[]
[null,"Hydro boiler"]
[]
[57,"5 litre Stainless steel water boiler , with stainless steel tank, steam free boiling water, electronic controls, 15mm overflow, connected to 15mm cold water supply including isolating valve and 230 volt 1800 watt electrical power supply, plugged and screwed to wall and fitted under 1 year warranty.",null,"No.",2]
[]
[null,"RAIN WATER GOODS"]
[]
[null,"0.8mm galvanized sheet iron"]
[]
[58,"125 x 100mm eaves gutter",null,"m",100]
[]
[59,"Extra over 125 x 100mm eaves gutter for stopped end",null,"No.",20]
[]
[60,"Extra over 125 x 100 eaves gutter for angle",null,"No.",25]
[]
[61,"Extra over 125 x 100mm eaves gutter for outlet for 100 x 75mm pipe",null,"No.",20]
[]
[62,"100 x 75mm rainwater pipes",null,"m",70]
[]
[63,"Extra over 100 x 75mm rainwater pipe for shoe",null,"No.",20]
[]
[null,"0.9mm galvanized sheet iron"]
[]
[64,"250 x 200mm industrial eaves gutter including heavy duty brackets fixed at 500mm centers",null,"m",100]
[]
[65,"Extra over 250 x 200mm eaves gutter for stopped end",null,"No.",10]
[]
[66,"Extra over 250 x 200 eaves gutter for angle",null,"No.",5]
[]
[67,"Extra over 125 x 100mm eaves gutter ",null,"No.",10]
[]
[68,"300mm rainwater pipes",null,"m",50]
[]
[69,"Extra over rainwater pipe for shoe",null,"No.",10]
[]
[{"$nulls":4},"Carried to final summary"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
["No."]
[]
[null,"BILL NO.9"]
[]
[null,"METAL WORK"]
[]
[null,"SECURITY GATES "]
[]
[null,"Supply and install Burglar door"]
[]
[1,"900 x 2100mm high Heavy duty Burglar door and frame with 16mm steel round bar and 40 x 40 x 2.5mm square tubing ",null,"No.",5]
[]
[2,"1500 x 2100mm high Heavy duty Burglar door and frame with 16mm steel round bar and 40 x 40 x 2.5mm square tubing ",null,"No.",1]
[]
[null,"Supply and install Burglar windows"]
[]
[3,"508mm W x 629mm H Box windows guard constructed with 5mm of expanded metal and 50 x 50 x 6mm equal angles.",null,"No.",10]
[]
[null,"Gates"]
[]
[null,"Gates welded to steel footbridge"]
[]
[4,"Supply and Install mild steel welded double swing gate 3m high x 4m wide steel swing gate with heavy duty hinges constructed from 76x50x3.5mm frame, diagonal intermediate steel section of 12x12mm at 100mm centers with heavy duty lock and bullet type hinges completely",null,"No.",2]
[]
[null,"Gates bolted to brickwork or concrete walls"]
[]
[5,"Supply and Install mild steel welded 3000mm high x 10000mm long steel sliding gate constructed from 120x60x4.5mm rectangular frame, intermediate steel section of 2 x 120x60x4.5mm and 1 x 120x60x4.5mm horizontal section including anti-lift system, heavy duty wheels and heavy duty lock completely with 16mm round bar diameter rail in trenches covered by 30 Mpa concrete",null,"No.",1]
[]
[null,"Steel flats sheets welded on gates and bugler doors"]
[]
[6,"3mm thick mild stainless steel plate sheets welded on gates and bugler doors on both sides",null,"m²",40]
[]
[{"$nulls":4},"Carried to final summary"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
[]
[null,"BILL NO.10"]
[]
[null,"GLAZING"]
[]
[null,"GLAZING TO STEEL WITH PUTTY"]
[]
[null,"38mm high penetration resistance clear laminated safety glass"]
[]
[1,"250 X 500mm high BRG viewing panel glazed in 38mm thick bullet resistant glass with one-way vision film",null,"No.",1]
[]
[null,"6.5mm high penetration resistance clear laminated safety glass"]
[]
[2,"Panes exceeding 0.1 m2 and not exceeding 0.5m2",null,"m²",8]
[]
[null,"4mm clear float glass"]
[]
[3,"Panes exceeding 0.1 m2 and not exceeding 0.5m2",null,"m²",20]
[]
[null,"4mm clear obscure glass"]
[]
[4,"Panes exceeding 0.1 m2 and not exceeding 0.5 m2",null,"m²",10]
[]
[null,"Mirrors"]
[]
[null,"6mm silver float glass copper backed mirrors with polished edges holed for and fixed with chromium plated dome capped mirror screws with rubber buffers to plugs in brickwork"]
[]
[5,"Mirror 1000 x 1000mm with four screws",null,"No.",5]
[]
[{"$nulls":4},"Carried to final summary"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
[]
[null,"BILL NO.11"]
[]
[null,"PAINTWORK"]
[]
[null,"For preambles see “Model Preambles for Trades” 2008 edition published by the Association of South African Quantity Surveyors "]
[]
[null,"SUPPLEMENTARY PREAMBLES"]
[]
[null,"Previously painted plastered surfaces "]
[]
[null,"Surfaces shall be thoroughly washed down and allowed to dry completely before any paint is applied. Blistered or peeling paint shall be completely removed and cracks shall be opened, filled with a suitable filler and finished smooth"]
[]
[null,"Previously painted metal surfaces "]
[]
[null,"Surfaces shall be thoroughly rubbed and cleaned down. Blistered or peeling paint shall be completely removed down to bare metal"]
[]
[null,"Previously painted wood surfaces "]
[]
[null,"Surfaces shall be thoroughly cleaned down. Blistered or peeling paint shall be completely removed and cracks and crevices shall be primed, filled with a suitable filler and finished smooth"]
[]
[null,"PAINTWORK, ETC TO NEW WORK"]
[]
[null,"ON FLOATED PLASTER"]
[]
[null,"One coat professional plaster primer and two coats of white Professional Superior Low Sheen  "]
[]
[1,"On ceiling and cornices ",null,"m²",200]
[]
[null,"ON WOOD"]
[]
[null,"One coat wood primer, one Universal Undercoat  and two coats Prasa Oakley Brown enamel paint"]
[]
[2,"On doors ",null,"m²",150]
[]
[null,"ON METAL"]
[]
[null,"One coat zinc chromate primer, one under coat  and two coats professional white gloss enamel paint"]
[]
[3,"On buglers, gates, door frames, window frames, rainwater goods etc",null,"m²",200]
[]
[null,"One coat professional plaster primer and two coats contractors Brick and Slasto Dressing/Brick seal"]
[]
[4,"On internal and external face brick walls   ",null,"m²",1000]
[]
[null,"PAINTWORK ETC TO PREVIOUSLY PAINTED WORK"]
[]
[null,"ON METAL"]
[]
[null,"Wash with polycell sugar soap and rinse with clean water to remove all traces of soap, remove all loose flaking paint and repair any cracks and defects, spot prime bare and repaired areas with bonding liquid and apply One coat of waterprime, one coat of universal undercoat, two coats of gloss Enamel of PRASA Grey \n"]
[]
[5,"On footbridge and all steel work",null,"m²",3000]
[]
[null,"ON FLOATED PLASTER"]
[]
[null,"Wash with polycell sugar soap and rinse with clean water to remove all traces of soap, remove all loose flaking paint and repair any cracks and defects, spot prime bare and repaired apply one coat sealer One coat primer, one under coat  and two coats PRASA Neutral"]
[]
[6,"On internal walls",null,"m²",1000]
[]
[null,"Wash with polycell sugar soap and rinse with clean water to remove all traces of soap, remove all loose flaking paint and repair any cracks and defects, spot prime bare and repaired areas with bonding liquid and apply one coat sealer and two coats of white Professional Superior Low Sheen  "]
[]
[7,"On ceiling",null,"m²",250]
[]
[null,"PLATFORM MARKING"]
[]
[null,"Prepare and paint yellow road marking paint on tared platform surfaces"]
[]
[8,"100mm wide yellow line",null,"m",2800]
[]
[{"$nulls":4},"Carried to final summary"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
[]
[null,"BILL NO.12"]
[]
[null,"MASONRY"]
[]
[null,"BRICKWORK"]
[]
[null,"20-30MPa Silver-gray Travertine or similar approved Imperial FBX clay face brick, size 222 x 106 x 73mm, manufactured in accordance with SANS 227:2007, bedded and jointed in Class I mortar and pointed with flush vertical, flush horizontal joints, with every 6th horizontal joint to be recessed. Brickwork of NFP bricks in class II mortar"]
[]
[null,"Bricks in Class II mortar"]
[]
[1,"One brick walls ",null,"m²",100]
[]
[null,"Brick reinforcement"]
[]
[2,"230mm wide reinforcement built in horizontal ",null,"m",150]
[]
[3,"Striking and Pointing on face brick work",null,"m²",250]
[]
[{"$nulls":4},"Carried to final summary"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
[]
[null,"BILL NO. 13"]
[]
[null,"PLASTERING"]
[]
[null,"SUPPLEMENTARY PREAMBLES "]
[]
[null,"Preparatory work for textured finishes:"]
[]
[null,"Textured finishes to be applied to plaster (plaster elsewhere )"]
[]
[null,"All surfaces are to be inspected and approved by Prasa representative before any work is commenced with "]
[]
[null,"Price for texture finishes:"]
[]
[null,"Prices are to include for all priming, preparatory work, etc"]
[]
[null,"One coat wood trowelled smooth cement plaster on brickwork"]
[]
[1,"On walls",null,"m²",150]
[]
[2,"On narrow widths",null,"m²",25]
[]
[null,"EXTERNAL PLASTER"]
[]
[3,"On walls",null,"m²",400]
[]
[4,"On narrow widths",null,"m²",25]
[]
[null,"(4:1) Cement screed to concrete floors "]
[]
[5,"25mm Thick screed to horizontal surfaces to receive ceramic tiles.",null,"m²",50]
[]
[{"$nulls":4},"Carried to final summary"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
[]
[null,"BILL NO. 14"]
[]
[null,"BLINDS"]
[]
[null,"Vertical blinds with 90mm slat width, colour to match walls and floor tiling"]
[]
[1,"Blinds to fit 2 x 2m high opening",null,"No.",15]
[]
[{"$nulls":4},"Carried to final summary"]
[]
[]
[]
[]
[]
[null,"CIVIL AND MINOR GENERAL WORKS FINAL SUMMARY"]
[]
[null,"Desctription",null,"Bill No.",{"$nulls":3},"Amount"]
[]
[]
[1,"Alterations",null,1,{"$nulls":3},"R"]
[]
[2,"Earth works",null,2,{"$nulls":3},"R"]
[]
[3,"Concrete works",null,3,{"$nulls":3},"R"]
[]
[4,"Roof covering",null,4,{"$nulls":3},"R"]
[]
[5,"Carpentry and Joinery",null,5,{"$nulls":3},"R"]
[]
[6,"Ceiling work",null,6,{"$nulls":3},"R"]
[]
[7,"Ironmongery",null,7,{"$nulls":3},"R"]
[]
[8,"Plumbing work",null,8,{"$nulls":3},"R"]
[]
[9,"Metal work",null,9,{"$nulls":3},"R"]
[]
[10,"Glazing",null,10,{"$nulls":3},"R"]
[]
[11,"Paint work",null,11,{"$nulls":3},"R"]
[]
[12,"Masonry",null,12,{"$nulls":3},"R"]
[]
[13,"Plastering",null,13,{"$nulls":3},"R"]
[]
[14,"Blinds",null,14,{"$nulls":3},"R"]
[]
[]
[]
[]
[null,"SUB TOTAL",{"$nulls":5},"R"]
[]
[null,"ADD VAT @ 15%",{"$nulls":5},"R"]
[]
[null,"TOTAL TENDER AMOUNT",{"$nulls":5},"R"]
{"$rows_empty":11}
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
[]
[null,"SECTION No. 3"]
[]
[null,"ELECTRICAL WORKS: SCHEDULE OF QUANTITIES"]
[]
[null,"PROVISIONAL SCHEDULE OF QUANTITIES "]
[]
[null,"Major Supply and Installation of Platform and Shelter Lighting at Midway Station"]
[]
[null,"BILL NO. 1"]
[]
[null,"ALTERATIONS (PROVISIONAL)"]
[]
[null,"REMOVAL OF EXISTING WORK"]
[]
[null,"Taking out and removing electrical work"]
[]
[1,"400W HPS fittings",null,"No.",6]
[]
[2,"Bulkhead fittings",null,"No.",50]
[]
[3,"4/5 foot fluorescent fittings",null,"No.",35]
[]
[{"$nulls":4},"Carried to final summary"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
[]
[null,"BILL NO.2"]
[]
[null,"ELECTRICAL WORK"]
[]
[null,"Supply, install test commission and hand over"]
[null,"in good working conditions complete the"]
[null,"electrical system as per BoQ, specifications, IEE wiring regulations & as required by Local Electrical Authorities (NEC) for the complete project all up to the Satisfaction of the Engineer. All the material to be supplied to bear SABS mark or SABS mark of compliance."]
[]
[null,"Fluorescent fittings waterproofed fixture white including 2x58w T8 LED Fluorescent tubes and polycarbonate base with clear polycarbonate cover IP65"]
[]
[1,"Waterproof polycarbonate LED 5ft 2 x58w T8 fluorescent fitting including 2 LED tubes",null,"No.",35]
[]
[2,"1200m (4 foot) 2x36w Open channel cool white LED Fluorescent fittings double tubes for ticket office building",null,"No.",25]
[]
[null,"Bulkhead fittings"]
[]
[3,"Corrosion resistance high pressure die- cast aluminium  LED 19w Bulkhead fitting with wire guard IP 65 bearing the SABS Mark minimum 50 000hrs lifetime 4 000K at a colour rendering index >70, injection moulded high impact acrylic diffuser  including opening tool for platform shelters",null,"No.",30]
[]
[null,"High colour rendering index CRI > 80, Colour temperature 4000K, 4710 lumens220-240V LED Module, -25 +800C, LM6 High pressure die cast aluminium body, Borosilicate dlear tempered glass, 316 stainless steel screws and heli-coils, 3 x 20mm diameter entry knockouts and 1 x M20 treaded gland entry"]
[]
[4,"410mmL x 271mmW x 120mmH B40 53W Bulkhead fitting, IP 65 bearing the SABS Mark minimum, 50 000hrs lamp service life, 50000hrs ECG Average life LM6 High pressure die cast aluminium body with high impact polycarbonate diffuser  LED Bulkhead fittings",null,"No.",20]
[]
[5,"7w LED bulk head  fittings completely with bulbs",null,"No.",15]
[]
[null,"HIGH BAY LED FITTINGS"]
[]
[null,"279W LED Lumminaire (34460 lumen) with 3 an optical compartment with LED engine, glass protector, LED warm light with colour temperature of 3000 kelvin, gear compartment and a spigot top entry adjustable compartment. Both optical and gear compartments to be rated IP 66. 20kV/kA surge protection. The luminaire housing to be manufactured of marine grade cast aluminium (EN 1706 AC-44300). Including 1 opening tool"]
[]
[null,"The use of cherry picker/scaffolder or any other equipment to be used for replacing of masts pole fittings and bulbs for the duration of the project"]
[]
[]
[6,"389 x 389 x 168mm 203W LED Lumminaire 32260 lumen) compartment with LED engine, glass protector, LED neutral white 740 with colour temperature of 4000 kelvin, Both optical and gear compartments to be rated IP 66. 10kV/kA surge protection. The luminaire housing to be manufactured of Marine grade high pressure die cast aluminium (EN 1706 AC 44300) optical housing Eco bay fittings to bears the SANS 60598 safety mark",null,"No.",5]
[]
[null,"High mast pole street light fitting"]
[]
[7,"279W LED Lumminaire (34460 lumen) with 3 an optical compartment with LED engine, glass protector, LED warm light with colour temperature of 3000 kelvin, gear compartment and a spigot top entry adjustable compartment. Both optical and gear compartments to be rated IP 66. 20kV/kA surge protection. The luminaire housing to be manufactured of marine grade cast aluminium (EN 1706 AC-44300). Including 1 opening tool",null,"No.",6]
[]
[8,"835x 345 x 35cm 265W LED MAXI light Lumminaire 43584 lumen)  with LED engine, glass protector, LED warm light with 730 colour temperature of 3000 kelvin, gear compartment and a spigot top entry adjustable compartment. Both optical and gear compartments to be rated IP 66. 20kV/kA surge protection. The luminaire housing to be manufactured of marine grade cast aluminium (EN 1706 AC-44300). Including 1 opening tool",null,"No.",18]
[]
[null,"SWITCHES"]
[]
[9,"Day light switches  ",null,"No.",4]
[]
[10,"11 kw contactors",null,"No.",3]
[]
[11,"White 1 lever 2 way switch",null,"No.",15]
[]
[12,"White 2 lever 1 way switch",null,"No.",6]
[]
[null,"Electrical cables"]
[]
[13,"70mm2 4 core armored cable in trenches measured else where  ",null,"m",100]
[]
[14,"25mm2 4 core armored cable in trenches measured else where  ",null,"m",450]
[]
[15,"16mm2 4 core armored cable in trenches measured else where  ",null,"m",300]
[]
[16,"10mm2 4 core armored cable in trenches measured else where  ",null,"m",500]
[]
[17,"4mm2 4 core armored cable in trenches measured else where  ",null,"m",150]
[]
[18,"2.5mm2  GP wires (Red, white, blue, black and earth) for lights rewiring of  shelters in 3 phase system",null,"m",400]
[]
[19,"2.5mm2 suffix cable or GP wire ",null,"m",200]
[]
[20,"1.5mm2 suffix cable or GP wire for lights",null,"m",200]
[]
[null,"Electrical casing"]
[]
[21,"20mm galvanized SABS conduit completely with all the couplings, galvanized saddle, spacer bar assembly and heavy duty U clamps completely encased 100mm deep on concrete walls and make good  ",null,"m",250]
[]
[22,"20mm PVC SABS conduit completely with all the couplings, saddle, spacer bar assembly and heavy duty U clamps",null,"m",100]
[]
[23,"40 x 25mm white heavy duty PVC trunking comlpetely with all the fittings",null,"m",50]
[]
[24,"76 x 76 X 0.8 mm galvanized  heavy duty steel trunking comlpetely with all the fittings",null,"m",30]
[]
[null,"PLUGS"]
[]
[25,"4 x 4 Double plug",null,"No.",10]
[]
[26,"4 x 4 single plug",null,"No.",10]
[]
[null,"Circuit breakers "]
[]
[27,"10 A 1P 6KA single circuit breaker",null,"No.",20]
[]
[28,"10 A 3P 6KA circuit breaker",null,"No.",5]
[]
[29,"12 A 3P Contactor",null,"No.",2]
[]
[30,"20 A 1P 6KA single circuit breaker",null,"No.",25]
[]
[31,"20 A 3P 6KA circuit breaker",null,"No.",3]
[]
[32,"30 A 1P 6KA circuit breaker",null,"No.",3]
[]
[33,"30 A 2P 6KA circuit breaker",null,"No.",3]
[]
[34,"40 A 2P 6KA circuit breaker",null,"No.",3]
[]
[35,"60 A 3P AC1 Contactor",null,"No.",2]
[]
[36,"63 A 2P 6KA circuit breaker",null,"No.",2]
[]
[37,"63 A 3P 6KA circuit breaker",null,"No.",2]
[]
[38,"63 A 30Ma 3P + N Earth leakage",null,"No.",2]
[]
[39,"400 A 3P Main circuit breaker",null,"No.",1]
[]
[40,"250 A 3P Main circuit breaker",null,"No.",2]
[]
[41,"80 A 3P Main circuit breaker",null,"No.",1]
[]
[42,"60 A 3P Main circuit breaker",null,"No.",1]
[]
[43,"40 A stove Isolator",null,"No.",1]
[]
[44,"30A Air conditioner  Isolator",null,"No.",2]
[]
[null,"DB BOARDS"]
[]
[45,"Surface mounted  min distribution board for staffroom (4 offices, one kitchen and 2 separate toilets )completely with circuit breakers",null,"No.",4]
[]
[46,"1000h x 400w x 400d x 2.0mm stainless steel orange IP 65 weatherproofed floor mounted lockable Station kiosk with 1 door completely rewired with all the circuit breakers mounted on din rail as per above and all other accessories, connected to the station",null,"No.",1]
[]
[47,"Lockable fiber glass water proofed 12 way CBI DB  Eaves box to be mounted on external walls for platform shelters, waiting areas, access point, ablutions, etc",null,"No.",15]
[]
[null,"HVAC Systems"]
[]
[48,"Supply, install and commission new 24000 BTU split unit, inverter technology air conditioner completely with all accessories (drain pipe, amorflex, copper pipe, refrigerant, cable, communication wire, brackets, circuit breaker, isolator, etc )",null,"No.",3]
[]
[null,"PLATFORM/STREET HIGH MAST STEEL POLES"]
[]
[null,"Pricing shall includes the design, supply, delivery to site, off-loading, erection, installation, commissioning, testing, and handing over in full working order a high mast lighting structure, including floodlight luminaries."]
[]
[null," The works specifically include the following: "]
[]
[null,"1. Geotechnical studies of proposed sites and issuing of soil test results. "]
[]
[null,"2. Design, preparation and cast of appropriate foundations. "]
[]
[null,"3. Design, supply, delivery to site, off-loading, erection, installation, commissioning, testing, and handing over in full working order a 30 meter high mast pole complete with Luminaries and control panel as specified."]
[]
[null,"4. Perform an electrical connection to the installation from the station kiosk"]
[]
[null,"5. Test and commissioning of the high mast lighting installation. "]
[]
[null,"6. Issuing of a certificate of compliance (COC) in terms of SANS 0142 Code of Practice.  "]
[]
[null,"7. all works should be accordance with the relevant specified specification (wirireing code SANS 0225)"]
[]
[null,"8. 30m high mast light shall be operated and maintaned in the horizontal position by means of a mechanical a mechanical winch "]
[]
[null," Tests "]
[]
[49,"Soil geotechnical studies for foundation including soil and concrete cube tests. ",null,"Per Pole",2]
[]
[50,"Perform soil bearing pressure tests for each mast prior to casting the concrete base to ensure that the soil load bearing conditions are suited to the specific concrete base design. Provide soil test Certificate ",null,"Per Pole",2]
[]
[51,"Test earth system and provide test certificate ",null,"Per Pole",2]
[]
[null,"Earth works"]
[]
[52,"Concrete foundation for high mast complete as per manufactrures specifications with excavation not exceeding 2m deep, steel reinforcing, cables inlet pipes, earth spikes, foundation bolts and template set, back fill material and soil concrete test.",null,"Per Pole",2]
[]
[null,"The use of Crane during the installation of 30m high mast poles"]
[]
[53,"Supply and deliver to site 30m above the ground HDG galvanized street pole with 9way Spiggot to recieve 9 lights per pole, LED Street lights priced elsewhere. Assemble and Erect complete with all accessories, distribution board, internal cables, carriage, earthing with 2 x earth spikesetc.  ",null,"No.",2]
[]
[null,"DOUBLE DRUM WORM WINCH "]
[]
[null,"H:328 MM, W:410mm, M:80kg "]
[]
[null,"Dymot DD800W Double drum Worm Winch "]
[]
[null,"S.W.L.: 800kg   (400kg +400kg) "]
[]
[null,"Rope DIA:6mm "]
[]
[null,"Drum Rope Capacity: 33m "]
[]
[null,"Gear Ratio:  50:1 "]
[]
[null,"Handle Radius:   285 "]
[]
[null,"Swive Base "]
[]
[null,"dia (7x19) Stainless Steel Rope Sling,  33 long "]
[]
[null,"C/W Stainless Thimble & Copper Ferule one end only. "]
[]
[null,"Power Tool "]
[]
[null,"220V Electric Power Tool "]
[]
[null,"c/w Torgue limiter & 3m remote cable "]
[]
[54,"Double Drum Worm Winch completely including, remote, Swive Base, power tools etc used for for lowered of high mast poles ",null,"No.",1]
[]
[null,"PIPE JACKING UNDER RAILWAY LINE"]
[]
[null,"HORIZONTAL DIRECTIONA DRILLING UNDER RAILWAY LINE AND INSTALLATION OF HDPE PIPE"]
[]
[55,"HDD under the railway lines and installation of 110mm diameter HDPE but welded on sleeve pipe with Nominal Pressure class 16 and material of PE100 to be used  including all fittings completely installed ",null,"m",100]
[]
[null,"SLEEVE"]
[]
[56,"110mm HDPE double wall corrugated coil with 5mm plain galvanized draw wire per sleeve. Both ends to be plugged before backfilling",null,"m",800]
[]
[null,"EARTHING"]
[]
[57,"Earth bonding (water pipes, stoves, etc)for the whole station as per SANS 10142 and"]
[null,"the specification.",null,"Item",1]
[]
[null,"ELECTRICAL COMPLIANCE"]
[]
[null,"All work to comply to SANS 10142"]
[null,"Compliance certificate to be provided on completion"]
[null,"Pricing to include all necessary complete connection"]
[]
[58,"Certificate of compliance and all other testing required including 12 month guarantee certificate"]
[]
[{"$nulls":4},"Carried to final summary"]
[]
["Item","Description",null,"Unit","Quantity","Rate",null,"Amount"]
[]
[null,"BILL NO. 3"]
[]
[null,"EARTHWORKS"]
[]
[null,"EXCAVATION, FILLING, ETC"]
[]
[1,"Removing and relaying of paving blocks after cables has been laid. To be relayed as per manufactures specification",null,"m²",750]
[]
[null,"Excavation in earth not exceeding 2m deep"]
[]
[null,"Trenches"]
[]
[null,"Earth filing obtain from the excavation and/or prescribed stock piles on site compacted to 90% Mod AASHTO density"]
[]
[2,"Backfilling to holes after concrete has been laid ",null,"m3",700]
[]
[null,"15 Mpa/20 mm unreinforced concrete"]
[]
[3,"1m long * 0.5m wide  x 0.2m thick Concrete block on every five meter interval on top of 16 mm² 4-core underground cable",null,"m3",20]
[]
[null,"Tar resurfacing"]
[]
[4,"Cutting of tar, Site preparations and apply 40mm thick Medium Hot Asphalt  ",null,"m²",100]
[]
[{"$nulls":4},"Carried to final summary"]
[]
[]
[]
[]
[]
[]
[null,"FINAL SUMMARY "]
[null,"ELECTRICAL WORK AT MIDWAY STATION"]
[]
[]
[null,"SECTION No.3"]
[]
[1,"ALTERATIONS",null,"BILL No.1",{"$nulls":3},"R"]
[]
[2,"ELECTRICAL WORK",null,"BILL No.2",{"$nulls":3},"R"]
[]
[3,"EARTHWORKS",null,"BILL No.3",{"$nulls":3},"R"]
[]
[]
[]
[]
[]
[null,"SUB TOTAL",{"$nulls":5},"R"]
[]
[null,"ADD VAT @ 15%",{"$nulls":5},"R"]
[]
[null,"TOTAL TENDER AMOUNT",{"$nulls":5},"R"]
[]
[]
[]
[]
[]
[]
[null,"FINAL SUMMARY "]
[null,"MINOR UPGRADES AT MIDWAY STATION"]
[]
[]
[]
[]
[1,"PRELIMINARY AND GENERAL ",null,"SECTION No.1",{"$nulls":3},"R"]
[]
[2,"CIVIL AND GENERAL BUILDING WORK AT MIDWAY STATION",null,"SECTION No.2",{"$nulls":3},"R"]
[]
[3,"ELECTRICAL WORK",null,"SECTION No.3",{"$nulls":3},"R"]
[]
[]
[]
[]
[null,"SUB TOTAL",{"$nulls":5},"R"]
[]
[null,"ADD VAT @ 15%",{"$nulls":5},"R"]
[]
[null,"TOTAL TENDER AMOUNT",{"$nulls":5},"R"]

{"sheet":"KLIPTOWN","index":3,"n_rows":151,"n_cols":6,"rows_kept":151,"flags":["formulas_cached_only"]}
[]
[null,"REFURBISHMENT OF KLIPTOWN STATION (Phase 1)- SOUTH GAUTENG REGION : RFQ NO:13/07/2022/05CRES","Unit","Quantity","Rate","Amount"]
[]
["ITEM NO","SECTION 1"]
[null,"BILL NO. 1"]
[null,"PRELIMINARIES"]
[null,"BUILDING AGREEMENT AND PRELIMINARIES"]
[]
[null,"The JBCC Series 2000 Principal Building Agreement (July 2007"]
[null,"edition 5.0) prepared by the Joint Building Contracts"]
[null,"Committee, shall be the agreement, amended as hereinafter"]
[]
[null,"The Preliminaries for use with the JBCC Series 2000 Principal"]
[null,"Building Agreement (May 2005 edition) prepared by the Joint"]
[null,"Building Contracts Committee, shall be deemed to be"]
[null,"incorporated in these bills of quantities"]
[null,"Contractors are referred to the above-mentioned documents for"]
[null,"the full intent and meaning of each clause thereof"]
[null,"These clauses are hereinafter referred to by clause number"]
[null,"and heading only. Where standard clauses or alternatives are"]
[null,"not entirely applicable to this contract such modifications,"]
[null,"corrections or supplements as will apply are given under each"]
[null,"relevant clause heading and such modifications, corrections or"]
[null,"supplements shall take precedence notwithstanding anything"]
[null,"contrary contained in the above-mentioned documents"]
[]
[]
[null,"SECTION A: PRINCIPAL BUILDING"]
[null,"AGREEMENT"]
[null,"1 Clause 1.0 - Definitions and interpretation "]
[null,"Interpretation (A1-A7)"]
[]
[null,"SECTION B: GENERAL PRELIMINARIES"]
[]
[1,"1. General Preliminaries to Include Appointment of Local CLO, site clearance of trees, shrubs, access vegitation and make good",{"$nulls":3},{"v":350000,"d":"R 350,000.00"}]
[]
[null,"SECTION NO. 2"]
[]
[null,"DEMOLITIONS ETC"]
[]
[null,"Allow R300 000.00 to include 7.5% attendance and handling fee for demolishing of existing structures and take off site,  then make good at platforms, Eastern and Western Ticket office, existing ablutions, existing retail area, unused stalls, Structural Steel, Old Steel Poles along the rails. ",null,"SUM "]
[2]
[null,"CONCRETE"]
[null,"Supply and fit concrete dust bins around the station 900mm long x 300mm diameter and make good.","NO",10]
[]
[null,"TICKET OFFICE"]
[]
[null,"Allow R750 000.00 to include 7.5% of attendance and handling fee to design, supply and full fitout of ticket office proposed for functionality. The proosal as per brief to have selling counter, Bullet Proof Window, Turnstiles, tiling, ceiling, etc. ",null,"Item "]
[]
[]
[null,"Guard room"]
[]
[null,"Allow R150 000.00 to refurbish 2 x Guard rooms to iclude 7.5% attendance and handling fee. ",null,"Item"]
[]
[]
[null,"SIGNAGE"]
[]
[null,"External signage"]
[]
[null,"500 x 150mm High double-sided ceiling mounted directional sign anodized aluminium female and male ablutions pictogram door sign, suspended from ceiling grids with brass chains. Minimum of 2,1m above finished floor level.","No.",2]
[]
[null,"Allow to supply and fit station signage "]
[]
[null,"Station name,  to match the existing","No ",2]
[]
[null,"Straight cutting"]
[null,"-----------------------------------------------------"]
[null,"PROFILED METAL SHEETING AND"]
[null,"ACCESSORIES"]
[null,"ON TICKET OFFICE"]
[null,"8 Roof covering with pitch not exceeding 25 degrees m² 344 320.00 110 080.00"]
[4,"0.58mm \"Klip Lok 700\" Z275 spelter galvanised"]
[null,"ribbed sheet steel with \"Chromadek\" finish on one (13.5m x 5m )","m2",67]
[null,"side in single lengths and accessories, fixed to"]
[null,"timber purlins using SL 700 approved clips and"]
[null,"fasteners all in accordance with manufacturer's recommendations and specifications."]
[]
[null,"PLUMBING AND DRAINAGE"]
[null,"Drainage and Water Connection"]
[null,"Allow R50 000.00 on all UPVC Pipes for drainage at Ablutions and Kitchen on existing buildings and Sewer connection as per below"]
[]
[null,"MANHOLE COVERS"]
[null,"Precast concrete manholes with medium duty concrete manhole cover and frame bedded in 1:3 cement mortar, spacers bedded in 1:6 cement mortar and precast concrete slab including excavation, backfilling, compaction, risk of collapse, cartaway surplus material, 300mm thick unreinforced 20MPa/19mm concrete base projection75mm wide from walls, benching, junctions, channeling and step irons  "]
[]
[null,"980mm diameter Precast concrete manhole cover including frame","No ",5]
[]
[null,"Sewer connection"]
[]
[null,"Cutting into sides of existing manhole chamber for and connecting 110mm pipe including inserting 110mm channel junction and making good concrete benching",null,"Item "]
[]
[null,"SECURITY GATES "]
[]
[null,"Supply and install Burglar door"]
[]
[null,"815 x 2100mm high Heavy duty Burglar door and frame with 16mm steel round bar and 40 x 40 x 2.5mm square tubing as per attached drawing for single door","no",4]
[]
[null,"STEEL ROLLER SHUTTERS "]
[]
[null,"Roll-Up solid galvanised, SABS 1461, & epoxy coated M/S manually hand chain operated push-up roller shutter for maximum opening 3000 x 3000mm high with standard bottom rail, 75 x 0.8mm thick end-locked slats, 120mm extra-wide tamper proof guides, 4.5mm end plates, closed shaft and 2 x slidebolts, extruded with Aluminium Tbar & Astragal rubber weather seal. Including galv. cover box and powder coated components incl. door curtain, end plates, cover box, guides & T-bar. Door fixed to brick, concrete or structural steel jambs and concrete or steel lintel over. Contractor to provide cavity of 160mm x 120mm for recessing guides"]
[]
[null,"Manual hand chain Push-up Roller Shutters, for openings not exceeding 3000mm x 2500mm high.","no",2]
[]
[null,"Supply and install Burglar windows"]
[null,"600mm W x 600mm H Box windows guard constructed with 5mm of expanded metal and 50 x 50 x 6mm equal angles. ",null,"SUM"]
[]
[null,"1200mm W x 600mm H Box windows guard constructed with 5mm of expanded metal and 50 x 50 x 6mm equal angles.",null,"SUM"]
[]
[null,"300mm W x 900mm H Box windows guard constructed with 5mm of expanded metal and 50 x 50 x 6mm equal angles.",null,"SUM"]
[]
[]
[null,"BRICKWALL AND GATES"]
[null,"Bricks shall have been obtained from an approved manufactured and shall be either general purpose (special) burn clay bricks or Engineering bricks that comply with the applicable requirements of SABS 285. The contractor shall submit to the project manager samples of the bricks that he/she intends using in the construction of the works. The sample of the bricks that are approved will be retained by the Project manager. See sub clause 3.1 of SABS 1200A or 1200AA as applicable"]
[null,"One double brick wall allow for access (Hieght 3m)","M",347]
[]
[null,"Supply and fit – replace heavy duty gate , with heavy duty industrial motor which allows to be operated manually also., allow all necessary fittings to be installed to the total completion","NO",2]
[]
[null,"Replace the electric fence around the wall and allow for the new connection and allow to the full completion of job."]
[]
[null,"BILL NO.12"]
[null,"PAINTWORK"]
[null,"Allow R250 000.00 for All paintwork internal and external walls , steel work, doors, etc ",null,"SUM"]
[null,"etc."]
[]
[null,"SECTION 3"]
[null,"ELECTRICAL WORK"]
[]
[null,"Allow R350 000.00 on Electrical Works and reticulation  to include all power supply to the station and connection from municipal supply to iclude but not limited to High mast pole street light fitting, The luminaire to consists of a separate lamp, control gear and spigot compartment. The control gear housing to be separated from the lamp housing for thermal reasons. To be designed to operate 70/400W mercury vapour and 70/400W high- pressure sodium/metal halide lamp. ",null,"SUM"]
[{"$nulls":3},{"v":3500,"d":"3,500"}]
[null,"PLATFORMS"]
[null,"Platform resurfacing with Asphalt and all Yellow Markings","m2",{"v":3500,"d":"3,500"}]
[]
[null,"PAVING"]
[null,"Allow R300 000. 00 with 7.5% for attendance and handling fee for preparing the surface to receive paver blocks as per PRASA spec ",null,"SUM"]
[]
[null,"STEEL WORK"]
[]
[null,"Allow R150 000.00 for bullustrade and handrails to staircases, include 7.5% handling and managent fee, all works to remeasured",null,"SUM"]
[]
[null," CONSTRUCTION COST"]
[]
[]
[null," FINAL SUMMARY"]
[null,"10 % Contingency fund"]
[]
[]
[]
[null,"SUB TOTAL"]
[]
[null,"ADD VAT @ 15%"]
[]
[null,"TOTAL AMOUNT "]

{"sheet":"NANCEFIELD ","index":4,"n_rows":144,"n_cols":6,"rows_kept":144,"flags":["formulas_cached_only"]}
[]
[null,"REFURBISHMENT OF NANCEFIELD STATION (Phase 1)- SOUTH GAUTENG REGION: RFQ NO: 13/07/2022/04CRES","Unit","Quantity","Rate","Amount"]
[]
["ITEM NO","SECTION 1"]
[null,"BILL NO. 1"]
[null,"PRELIMINARIES"]
[null,"BUILDING AGREEMENT AND PRELIMINARIES"]
[]
[null,"The JBCC Series 2000 Principal Building Agreement (July 2007"]
[null,"edition 5.0) prepared by the Joint Building Contracts"]
[null,"Committee, shall be the agreement, amended as hereinafter"]
[]
[null,"The Preliminaries for use with the JBCC Series 2000 Principal"]
[null,"Building Agreement (May 2005 edition) prepared by the Joint"]
[null,"Building Contracts Committee, shall be deemed to be"]
[null,"incorporated in these bills of quantities"]
[null,"Contractors are referred to the above-mentioned documents for"]
[null,"the full intent and meaning of each clause thereof"]
[null,"These clauses are hereinafter referred to by clause number"]
[null,"and heading only. Where standard clauses or alternatives are"]
[null,"not entirely applicable to this contract such modifications,"]
[null,"corrections or supplements as will apply are given under each"]
[null,"relevant clause heading and such modifications, corrections or"]
[null,"supplements shall take precedence notwithstanding anything"]
[null,"contrary contained in the above-mentioned documents"]
[]
[]
[null,"SECTION A: PRINCIPAL BUILDING"]
[null,"AGREEMENT"]
[null,"1 Clause 1.0 - Definitions and interpretation "]
[null,"Interpretation (A1-A7)"]
[]
[null,"SECTION B: GENERAL PRELIMINARIES"]
[]
[1,"1. General Preliminaries to Include Appointment of Local CLO, site clearance of trees, shrubs, access vegitation and make good",{"$nulls":3},{"v":350000,"d":"R 350,000.00"}]
[]
[null,"SECTION NO. 2"]
[]
[null,"DEMOLITIONS ETC"]
[]
[null,"Allow R450 000.00 to include 7.5% attendance and handling fee for demolishing of existing structures and take off site,  then make good at platforms, Eastern and Western Ticket office, existing ablutions, existing retail area, unused stalls, Structural Steel, Old Steel Poles along the rails. ",null,"SUM "]
[2]
[null,"CONCRETE"]
[null,"Supply and fit concrete dust bins around the station 900mm long x 300mm diameter and make good.","NO",10]
[]
[null,"TICKET OFFICE"]
[]
[null,"Allow R500 000.00 to include 7.5% of attendance and handling fee to design, supply and full fitout of ticket office proposed for functionality. The proosal as per brief to have selling counter, Bullet Proof Window, Turnstiles, tiling, ceiling, etc. ",null,"Item "]
[]
[null,"SIGNAGE"]
[]
[null,"External signage"]
[]
[null,"500 x 150mm High double-sided ceiling mounted directional sign anodized aluminium female and male ablutions pictogram door sign, suspended from ceiling grids with brass chains. Minimum of 2,1m above finished floor level.","No.",2]
[]
[null,"Allow to supply and fit station signage "]
[]
[null,"Station name,  to match the existing","No ",2]
[]
[null,"Straight cutting"]
[null,"-----------------------------------------------------"]
[null,"PROFILED METAL SHEETING AND"]
[null,"ACCESSORIES"]
[null,"ON TICKET OFFICE (Re-measure)"]
[null,"8 Roof covering with pitch not exceeding 25 degrees m² 344 320.00 110 080.00"]
[4,"0.58mm \"Klip Lok 700\" Z275 spelter galvanised"]
[null,"ribbed sheet steel with \"Chromadek\" finish on one (13.5m x 5m )","m2",67]
[null,"side in single lengths and accessories, fixed to"]
[null,"timber purlins using SL 700 approved clips and"]
[null,"fasteners all in accordance with manufacturer's recommendations and specifications."]
[]
[null,"PLUMBING AND DRAINAGE"]
[null,"Drainage and Water Connection"]
[null,"Allow R50 000.00 on all UPVC Pipes for drainage at Ablutions and Kitchen on existing buildings and Sewer connection as per below"]
[]
[null,"MANHOLE COVERS"]
[null,"Precast concrete manholes with medium duty concrete manhole cover and frame bedded in 1:3 cement mortar, spacers bedded in 1:6 cement mortar and precast concrete slab including excavation, backfilling, compaction, risk of collapse, cartaway surplus material, 300mm thick unreinforced 20MPa/19mm concrete base projection75mm wide from walls, benching, junctions, channeling and step irons  "]
[]
[null,"980mm diameter Precast concrete manhole cover including frame","No ",5]
[]
[null,"Sewer connection"]
[]
[null,"Cutting into sides of existing manhole chamber for and connecting 110mm pipe including inserting 110mm channel junction and making good concrete benching",null,"Item "]
[]
[null,"SECURITY GATES "]
[]
[null,"Supply and install Burglar door"]
[]
[null,"815 x 2100mm high Heavy duty Burglar door and frame with 16mm steel round bar and 40 x 40 x 2.5mm square tubing as per attached drawing for single door","no",4]
[]
[null,"STEEL ROLLER SHUTTERS "]
[]
[null,"Roll-Up solid galvanised, SABS 1461, & epoxy coated M/S manually hand chain operated push-up roller shutter for maximum opening 3000 x 3000mm high with standard bottom rail, 75 x 0.8mm thick end-locked slats, 120mm extra-wide tamper proof guides, 4.5mm end plates, closed shaft and 2 x slidebolts, extruded with Aluminium Tbar & Astragal rubber weather seal. Including galv. cover box and powder coated components incl. door curtain, end plates, cover box, guides & T-bar. Door fixed to brick, concrete or structural steel jambs and concrete or steel lintel over. Contractor to provide cavity of 160mm x 120mm for recessing guides"]
[]
[null,"Manual hand chain Push-up Roller Shutters, for openings not exceeding 3000mm x 2500mm high.","no",2]
[]
[null,"Supply and install Burglar windows"]
[null,"600mm W x 600mm H Box windows guard constructed with 5mm of expanded metal and 50 x 50 x 6mm equal angles. ",null,"SUM"]
[]
[null,"1200mm W x 600mm H Box windows guard constructed with 5mm of expanded metal and 50 x 50 x 6mm equal angles.",null,"SUM"]
[]
[null,"300mm W x 900mm H Box windows guard constructed with 5mm of expanded metal and 50 x 50 x 6mm equal angles.",null,"SUM"]
[]
[]
[null,"FENCE AND GATES"]
[]
[null,"Supply and Install Unobtrusive Clear view fence or similar approved with Polyester Coated Black, Apertures (76mm x 12.7 mm), Anti-Cut & Grind (Impenetrable meshing) and anti climb feature of 3m high including spikes ","m",151]
[]
[null,"Supply and fit – replace heavy duty gate , with heavy duty industrial motor which allows to be operated manually also., allow all necessary fittings to be installed to the total completion of the job.","no",2]
[]
[]
[null,"BILL NO.12"]
[null,"PAINTWORK"]
[null,"Allow R250 000.00 for All paintwork internal and external walls , steel work, doors, etc ",null,"SUM"]
[null,"etc."]
[]
[null,"SECTION 3"]
[null,"ELECTRICAL WORK"]
[]
[null,"Allow R350 000.00 on Electrical Works and reticulation  to include all power supply to the station and connection from municipal supply to iclude but not limited to High mast pole street light fitting, The luminaire to consists of a separate lamp, control gear and spigot compartment. The control gear housing to be separated from the lamp housing for thermal reasons. To be designed to operate 70/400W mercury vapour and 70/400W high- pressure sodium/metal halide lamp. ",null,"SUM"]
[{"$nulls":3},{"v":3500,"d":"3,500"}]
[null,"PLATFORMS"]
[null,"Prepare platforms to receive Asphalt(Resurfacing) to include all Yellow Markings","m2",{"v":3500,"d":"3,500"}]
[]
[null,"PAVING"]
[null,"Allow R300 000. 00 with 7.5% for attendance and handling fee for preparing the surface to receive paver blocks as per PRASA spec (for both East and West )",null,"SUM"]
[]
[null,"STEEL WORK"]
[]
[null,"Allow R150 000.00 for bullustrade and handrails to staircases, include 7.5% handling and managent fee, all works to remeasured",null,"SUM"]
[]
[null," CONSTRUCTION COST"]
[]
[]
[null," FINAL SUMMARY"]
[null,"10 % Contingency fund"]
[]
[]
[]
[null,"SUB TOTAL"]
[]
[null,"ADD VAT @ 15%"]
[]
[null,"TOTAL AMOUNT "]

{"sheet":"ORLANDO","index":5,"n_rows":263,"n_cols":6,"rows_kept":263,"flags":["formulas_cached_only"]}
[]
[null,"REFURBISHMENT OF OLANDO STATION (Phase 1)- SOUTH GAUTENG REGION: RFQ NO: 13/07/2022/03CRES","Unit","Quantity","Rate","Amount"]
[]
["ITEM NO","SECTION 1"]
[null,"BILL NO. 1"]
[null,"PRELIMINARIES"]
[null,"BUILDING AGREEMENT AND PRELIMINARIES"]
[]
[null,"The JBCC Series 2000 Principal Building Agreement (July 2007"]
[null,"edition 5.0) prepared by the Joint Building Contracts"]
[null,"Committee, shall be the agreement, amended as hereinafter"]
[]
[null,"The Preliminaries for use with the JBCC Series 2000 Principal"]
[null,"Building Agreement (May 2005 edition) prepared by the Joint"]
[null,"Building Contracts Committee, shall be deemed to be"]
[null,"incorporated in these bills of quantities"]
[null,"Contractors are referred to the above-mentioned documents for"]
[null,"the full intent and meaning of each clause thereof"]
[null,"These clauses are hereinafter referred to by clause number"]
[null,"and heading only. Where standard clauses or alternatives are"]
[null,"not entirely applicable to this contract such modifications,"]
[null,"corrections or supplements as will apply are given under each"]
[null,"relevant clause heading and such modifications, corrections or"]
[null,"supplements shall take precedence notwithstanding anything"]
[null,"contrary contained in the above-mentioned documents"]
[]
[]
[null,"SECTION A: PRINCIPAL BUILDING"]
[null,"AGREEMENT"]
[null,"1 Clause 1.0 - Definitions and interpretation "]
[null,"Interpretation (A1-A7)"]
[]
[null,"SECTION B: GENERAL PRELIMINARIES"]
[]
[1,"1. General Preliminaries to Include Appointment of Local CLO, site clearance of trees, shrubs, access vegitation and make good",{"$nulls":3},{"v":350000,"d":"R 350,000.00"}]
[]
[null,"SECTION NO. 2"]
[]
[null,"DEMOLITIONS ETC"]
[]
[null,"Allow R100 000.00 to include 7.5% attendance and handling fee for demolishing of existing structures and take off site,  then make good at platforms, Old Western Ticket office, existing ablutions, existing retail area, unused stalls, Structural Steel, Old Steel Poles along the rails. "]
[]
[null,"CARPENTRY AND JOINERY"]
[]
[null,"CEILING WORK"]
[]
[null,"SUPPLEMENTARY PREAMBLES "]
[]
[null,"Description "]
[]
[null,"Items described as “nailed” shall be deemed to be fixed with hardened steel nails or pins or shot pinned to brickwork or concrete"]
[]
[null,"Items described as “plugged” shall be deemed to include screwing to fibre, plastic or metal plugs at not exceeding 600mm centres, and where described as “bolted”, bolts priced elsewhere"]
[]
[null,"6.4mm “Rhino” gypsum plaster board with H-Type pressed steel jointing strips"]
[]
[null,"Ceiling including 38 x 38mm sawn softwood brandering at 450mm centres","m2",120]
[]
[null,"Extra over ceiling for 800 x 800mm trap door of 38 50mm wrought softwood rebated framing with one 38 x 38mm sawn softwood cross brander covered with ceiling board and fitted flush in opening","No.",2]
[]
[null,"“Rhino” gypsum plasterboard cornice"]
[]
[null,"75mm coved cornices","m2",126]
[]
[null,"Allow for Eave closures around the station ",null,"SUM"]
[]
[null,"IRONMONGERY"]
[]
[null,"LOCKS"]
[]
[null,"3 liver union lock with handles ","No.",2]
[]
[null,"Ultra-security heavy duty locks","No.",2]
[]
[null,"Stainless Steel Toilet Cubicle Indicator bolt & lock set, Grade 304Stainless Steel indicator bolt fixed to surface with matching stainless-steel screws.","No.",4]
[]
[null,"Satin stainless-steel toilet roll holders for 2 rolls with central shaft system and cylinder lock, plugged and screwed to the wall with stainless steel screws. (vandal resistant)","No",4]
[]
[null,"SIGNAGE"]
[]
[null,"External signage"]
[]
[null,"500 x 150mm High double-sided ceiling mounted directional sign anodized aluminium female and male ablutions pictogram door sign, suspended from ceiling grids with brass chains. Minimum of 2,1m above finished floor level.","No.",4]
[]
[]
[null,"TILING"]
[]
[null,"Prices:"]
[]
[null,"Prices are to include for all square cutting and waste, cleaning off on completion and protection from injury. Areas are measured net to face of brickwork and concrete. Any additional area caused by the thickness of tiling and screed are to be allowed for in prices "]
[]
[null,"FLOOR TILING"]
[]
[null,"600x600mm Full Bodied polished Porcelain tiles with 3mm grouting lines"]
[]
[null,"On floors","m2",20]
[]
[null,"WALL TILING"]
[]
[null,"Matt Full Bodied Porcelain tiles, size 600 x 300mm x 12mm fixed to internal wall plaster backing with TAL tile adhesive mixed with TAL bonding liquid in lieu of water with joints continuous in both directions and grouted with TAL tile grout, excess grout on the surface to be cleaned with water as work proceeds."]
[]
[null,"On walls","m2",10]
[]
[null,"300x300x6mm Full Bodied polished Porcelain mosaic tiles with 3mm grouting lines"]
[]
[null,"On walls","m2",5]
[]
[null,"BILL NO. 2"]
[null,"ROOF COVERINGS ETC"]
[null,"ALLOW FOR REFURBISHMENT OF THE ROOF, GUTTERS, DOWN PIPES, ETC FOR AN AMOUNT OF R100 000.00 TO INCLUDE ALL WATERPROOFING REQUIREMENTS"]
[]
[null,"BILL NO. 3"]
[null,"PLUMBING AND DRAINAGE"]
[null,"SANITARY FITTINGS"]
[null,"ALLOW to reinstate   all sanitary fittings and plumbing in the station"]
[null,"Vaal Sanitary ware Hibiscus vitreous china close coupled suite colour White , comprising 90º outlet open rim pan with matching 9 litre front single flush cistern including lid and fitments and Jazz Thermoset seat."]
[]
[null,"Vaal Sanitary ware Hibiscus vitreous china lavatory basin colour White, size 510 x 405mm with two tap hole including integrated overflow and chain stay hole bolted to wall with two x 10mm bolts and including Classic floor mounted pedestal and sealed with silicone sealant where basin meets wall."]
[]
[null,"Top entry ceramic urinal basin with Junior flush master exposed chrome flush valve including flush pipe, spreader, etc"]
[null,"ALLOW as per below"]
[null,"WASTE UNINON ETC"]
[]
[null,"Bath and Basin waste, plug, chain, stay and backnut  "]
[]
[null,"TRAPS ETC"]
[]
[null,"365/40 CP bottle trap 40 x 40 INC CP/PVC adaptor to 40mm"]
[]
[null,"38mm sink “P” trap"]
[]
[null,"Brass shower P trap with square ss grating"]
[]
[null,"SINK, BASIN, ETC"]
[]
[null,"90Mm Bsw 1200x500x180mm double bowl Kitchen stainless steel sink"]
[]
[null,"TAPS, VALVES, ETC"]
[]
[null,"Kitchen sink Mixer taps"]
[]
[null,"Push button pillar tap for hot and cold water"]
[]
[null,"Flexi connector"]
[]
[null,"15 Mini Ball Valve "]
[]
[null,"WATER SUPPLIERS"]
[null,"Allow reconnection of water for  R150 000.00 using Class “O” copper pipes "]
[]
[]
[null,"ELECTRIC WATER HEATERS"]
[]
[null,"Supply, deliver and install Electrical geysers with all other accessories  "]
[]
[null,"250L 600i dual electric water heater Geyser completely with safety valve, drain cock, vacuum breaker, gate valve, 1350 x 650mm tray and pressure regulating valve.","No",1]
[]
[]
[null,"Manhole covers and grid inlets"]
[]
[null,"560mm wide x 65mm thick heavy duty polymer grid inlet including frame","no ",5]
[]
[null,"SOIL DRAINAGE"]
[null,"Allow R100 000.00 on all UPVC Pipes for drainage at Ablutions and Kitchen on existing buildings and Sewer connection as per below"]
[]
[null,"Upvc waste pipes"]
[]
[null,"50mm pipes with all connection and make good ","no",5]
[]
[null,"Upvc class 34 pipes including excavation, bedding, backfilling and compaction and disposal of surplus material"]
[]
[null,"110mm pipes vertical or ramped to cleaning eyes etc (no excavation)","no",10]
[]
[null,"110mm pipes laid in and including trenches not exceeding 1m deep","no",10]
[]
[null,"50mm pipes with all connection and make good","no",10]
[]
[null,"Extra over Upvc class 34 pipes for fittings"]
[]
[null,"110 Bend","no",5]
[]
[null,"110mm junction","no",5]
[]
[null,"110mm Access bend","no",5]
[]
[null,"Upvc Gulley","no",5]
[]
[null,"110mm Gulley not exceeding 1m deep formed of trap, vertical pipe and gully head with loose grating, encased in 15MPa unreinforced concrete, with top of gully 50mm above surrounding finished surfaces, top surface of concrete splayed and with 1:3 cement plaster on exposed surfaces"]
[]
[null,"Sundries"]
[]
[null,"110mm Upvc cleaning eye to end of 110 Upvc pipe","no",5]
[]
[null,"350 x 350 x 50mm thick precast concrete inspection eye marker slab finished smooth on exposed surfaces with letters “I.E” or “I.O” on top and placed flush in ground or paving","no",6]
[]
[null,"Testing soil drainage system "]
[]
[null,"Manhole covers"]
[]
[null,"Precast concrete manholes with medium duty concrete manhole cover and frame bedded in 1:3 cement mortar, spacers bedded in 1:6 cement mortar and precast concrete slab including excavation, backfilling, compaction, risk of collapse, cartaway surplus material, 300mm thick unreinforced 20MPa/19mm concrete base projection75mm wide from walls, benching, junctions, channeling and step irons  "]
[]
[]
[null,"980mm diameter Precast concrete manhole cover including frame","no",6]
[]
[null,"Sewer connection"]
[]
[null,"Cutting into sides of existing manhole chamber for and connecting 110mm pipe including inserting 110mm channel junction and making good concrete benching"]
[]
[null,"WATER RETICULATION"]
[]
[null,"PREMBLES"]
[]
[null,"The contractor is referred to the General Preambles for trades 2017 published by the Association of South Africa Quantity Surveyors before pricing"]
[]
[null,"WATER PIPEWORK"]
[]
[null,"HDPE PE 100PN 12.5 pipes including excavation, bedding, backfilling, and compaction and disposal of surplus material"]
[]
[null,"25mm pipes laid in and including trenches not exceeding 1m deep"]
[]
[null,"Extra over HDPE"]
[]
[null,"25mm elbow","no",3]
[]
[null,"25mm equal tee","no",2]
[]
[null,"25mm couplings pipe connectors ","no",3]
[]
[null,"Fire hydrant system around the station building and platform","no",6]
[]
[]
[null,"Allow to supply and fit complete paraplegic toilet system including all necessary fittings and make good."]
[{"$nulls":3},"SUM"]
[null,"MIRROR"]
[]
[null,"6.5mm silvered float glass copper backed mirrors with polished adges holed for and fixed with chromium plated dome capped mirror screws with rubber buffers to plugs in brickwork "]
[]
[null,"Mirror 600 x 1200mm high with four screws ","no",7]
[]
[null,"Ticket window with window frame and bullet proof with prasa  full spec.","no",7]
[]
[]
[null,"PAINTWORK"]
[]
[null,"Allow R350 000.00 for All paintwork internal and external walls , steel work, doors, etc ",null,"SUM"]
[]
[null,"SECTION 3"]
[null,"ELECTRICAL WORK"]
[]
[null,"Allow R500 000.00 on Electrical Works and reticulation  to include all power supply to the station and connection from municipal supply to iclude but not limited to High mast pole street light fitting, The luminaire to consists of a separate lamp, control gear and spigot compartment. The control gear housing to be separated from the lamp housing for thermal reasons. To be designed to operate 70/400W mercury vapour and 70/400W high- pressure sodium/metal halide lamp. ",null,"SUM"]
[null," CONSTRUCTION COST"]
[]
[]
[null," FINAL SUMMARY"]
[null,"10 % Contingency fund"]
[]
[]
[]
[null,"SUB TOTAL"]
[]
[null,"ADD VAT @ 15%"]
[]
[null,"TOTAL AMOUNT "]

{"sheet":"MLAMLANKUNZI","index":6,"n_rows":748,"n_cols":6,"rows_kept":748,"merged":[[102,1,103,1],[102,2,103,2],[102,3,103,3],[102,4,103,4],[102,5,103,5],[106,1,107,1],[106,2,107,2],[106,3,107,3],[106,4,107,4],[106,5,107,5],[108,1,109,1],[108,2,109,2],[108,3,109,3],[108,4,109,4],[108,5,109,5],[110,1,111,1],[110,2,111,2],[110,3,111,3],[110,4,111,4],[110,5,111,5],[112,1,113,1],[112,2,113,2],[112,3,113,3],[112,4,113,4],[112,5,113,5],[153,2,156,2],[153,3,156,3],[153,4,156,4],[153,5,156,5],[159,2,161,2],[159,3,161,3],[159,4,161,4],[159,5,161,5],[258,1,259,1],[258,2,259,2],[258,3,259,3],[258,4,259,4],[258,5,259,5],[466,2,467,2],[466,3,467,3],[466,4,467,4],[466,5,467,5],[522,1,523,1],[522,2,523,2],[522,3,523,3],[522,4,523,4],[522,5,523,5],[528,2,529,2],[528,3,529,3],[528,4,529,4],[528,5,529,5],[549,2,559,2],[549,3,559,3],[549,4,559,4],[549,5,559,5],[563,2,565,2],[563,3,565,3],[563,4,565,4],[563,5,565,5]],"flags":["formulas_cached_only"]}
[]
[null,"REFURBISHMENT OF MLAMLANKUNZI (Phase 1)- SOUTH GAUTENG REGION:RFQ NO: 13/07/2022/02CRES","Unit","Quantity","Rate","Amount"]
[]
["ITEM NO","SECTION 1"]
[null,"BILL NO. 1"]
[null,"PRELIMINARIES"]
[null,"BUILDING AGREEMENT AND PRELIMINARIES"]
[]
[null,"The JBCC Series 2000 Principal Building Agreement (July 2007"]
[null,"edition 5.0) prepared by the Joint Building Contracts"]
[null,"Committee, shall be the agreement, amended as hereinafter"]
[]
[null,"The Preliminaries for use with the JBCC Series 2000 Principal"]
[null,"Building Agreement (May 2005 edition) prepared by the Joint"]
[null,"Building Contracts Committee, shall be deemed to be"]
[null,"incorporated in these bills of quantities"]
[null,"Contractors are referred to the above-mentioned documents for"]
[null,"the full intent and meaning of each clause thereof"]
[null,"These clauses are hereinafter referred to by clause number"]
[null,"and heading only. Where standard clauses or alternatives are"]
[null,"not entirely applicable to this contract such modifications,"]
[null,"corrections or supplements as will apply are given under each"]
[null,"relevant clause heading and such modifications, corrections or"]
[null,"supplements shall take precedence notwithstanding anything"]
[null,"contrary contained in the above-mentioned documents"]
[]
[]
[null,"SECTION A: PRINCIPAL BUILDING"]
[null,"AGREEMENT"]
[null,"1 Clause 1.0 - Definitions and interpretation "]
[null,"Interpretation (A1-A7)"]
[]
[null,"SECTION B: GENERAL PRELIMINARIES"]
[]
[1,"1. General Preliminaries to Include Appointment of Local CLO ",{"$nulls":3},{"v":350000,"d":"R 350,000.00"}]
[]
[null,"SECTION NO. 2"]
[]
[null,"BILL NO. 1","Unit","QTY","Rate","Amount"]
[]
[null,"ALTERATIONS (PROVISIONAL)"]
[2]
[null,"REMOVAL OF EXISTING WORK"]
[]
[]
[3,"Taking out and removing piping, sanitary fittings, etc including disconnection piping from fittings"]
[]
[null,"Pan and cistern  ","No.",6,"R               -","R                    -"]
[]
[null,"Kitchen sink cabinet","No.",2,"R               -","R                    -"]
[]
[null,"Ceramic wash hand basin ","No.",4,"R               -","R                    -"]
[]
[]
[null,"Taking out and removing doors including ironmongery and steel frame from walls"]
[]
[null,"Timber single door frame 813x2032mm high ","No.",3,"R               -","R                    -"]
[]
[null,"Taking up and removing floor covering"]
[4]
[null,"Vinyl tile/ceramic floor covering/mosaic floor tile/skirting including preparing screed to receive new floor tiling","m2",30,"R               -","R                    -"]
[]
[null,"Hacking up/off and removing ceramic wall tile"]
[]
[null,"Tiles to walls","m2",15,"R               -","R                    -"]
[]
[null,"Taking out and removing roller doors from brick walls "]
[]
[5,"2500 x 2100mm high from one brick wall","No.",6,"R               -","R                    -"]
[]
[]
[null,"4000 x 2100mm high from one brick wall","No.",2,"R               -","R                    -"]
[]
[6,"Taking out and removing roof sheets "]
[]
[null,"Corrugated side roof sheeting"]
[null,"Clean down existing face brick façade, painted walls, etc with water and brush"]
[]
[null,"External face brick walls ","m2",150,"R               -","R                    -"]
[]
[null,"Taking down and removing from site"]
[]
[null,"Torch on waterproofing membrane on concrete roof","m2",50,"R               -","R                    -"]
[]
[null,"Dig out and remove loose asphalt at the platform area allow to dump at the nearest approved dumping site.","m2",2400,"R               -","R                    -"]
[]
[null,"Dig out and remove debris , allow to dump at the nearest approved dumping site.","m2",100,"R               -","R                    -"]
[]
[null,"Dig out and remove loose soil and loose paving bricks","m2",50,"R               -","R                    -"]
[]
[null,"BILL NO 2","Unit","QTY","Rate","Amount"]
[]
[null,"EARTHWORKS"]
[]
[null,"SUPPLEMENTARY AND PREAMBLES"]
[]
[null,"Excavation:"]
[]
[null,"No claim for rock excavation will be entertain unless the contractor has timeously notified the project manager thereof prior to backfilling"]
[]
[null,"Laying, backfilling, bedding, etc"]
[]
[null,"Pipes shall be laid and bedded and trenches shall be carefully backfilled in accordance with manufacturers' instruction"]
[]
[null,"Where no manufacturers' instruction exist pipes shall be laid in accordance with clauses 5.1 and 5.2 of SABS 1200 L"]
[]
[null,"Pipe trenches etc shall be backfilled in accordance with clauses 3, 5.5, 5.6, 5.7, and 7 of SABS 1200 DB Earthworks (Pipe trenches)"]
[]
[null,"Pipes shall be bedded in accordance with clauses 3.1 to 3.4.1, 5.1 to 5.3  and 7 of SABS 1200  LB : Bedding (Pipes) "]
[]
[null,"Leave site in good condition   "]
[]
[null,"The contractor shall leave the site where plumbing was executed, clean and neat at completion."]
[]
[null,"EXCAVATION, FILLING, ETC"]
[]
[null,"Excavation in earth not exceeding 1m deep by hand"]
[]
[null,"Trenches and removing top soil at the platform ","m3",2000,"R                -","R                           -"]
[]
[]
[null,"Earth filling obtain from the excavation and/or prescribed stock piles on site compacted to 93% Mod AASHTO before and after bedding, final backfilling, etc"]
[]
[null,"100mm Bedding after compaction of underground surfaces","m2",2500,"R                -","R                           -"]
[]
[null,"Compaction of surfaces"]
[]
[null,"Compaction of ground surface under floors etc to 93% Mod AASHTO density ","m2",2500,"R                -","R                           -"]
[]
[null,"Cut to spoil or stockpile, site to be located by the contractor"]
[]
[null,"Material obtained from"]
[]
[null,"Lay down asphalt 100mm thick and allow all material to the full completion of the work.","m3",2500,"R                -","R                           -"]
[null,"BILL NO 3"]
[]
[null,"MASONRY"]
[]
[null,"Bricks shall have been obtained from an approved manufactured and shall be either general purpose (special) burn clay bricks or Engineering bricks that comply with the applicable requirements of SABS 285. The contractor shall submit to the project manager samples of the bricks that he/she intends using in the construction of the works. The sample of the bricks that are approved will be retained by the Project manager. See sub clause 3.1 of SABS 1200A or 1200AA as applicable"]
[]
[]
[null,"SUPERSTRUCTURE"]
[null,"20-30MPa Silver-gray Travertine or similar approved Imperial FBX clay face brick, size 222 x 106 x 73mm, manufactured in accordance with SANS 227:2007, bedded and jointed in Class I mortar and pointed with flush vertical, flush horizontal joints, with every 6th horizontal joint to be recessed. "]
[]
[null,"One brick walls","m2",20,"R                -","R                           -"]
[]
[null,"Supply and fit concrete dust bins around the station 900mm long x 300mm diameter and make good.","No ",20,"R                -","R                           -"]
[null,"BILL NO 4"]
[]
[null,"CARPENTRY AND JOINERY"]
[]
[null,"DOORS"]
[]
[null,"44mm thick interior grade flush solid core timber single door with 3 mm thick commercial"]
[null,"ply on both sides with consolidated edges fitted and complying with SABS 545 in pressed"]
[null,"steel frame. All painted in accordance with architects colour schedule."]
[]
[null,"813 x 2032 x 44mm single interior leaf solid core ","No.",10,"R                -","R                    -"]
[]
[null,"44mm thick exterior grade flush solid core timber single door with 3mm thick commercial"]
[null,"ply on both sides with consolidated edges fitted and complying with SABS 545 in pressed"]
[null,"steel frame. All painted in accordance with architect's colour schedules "]
[]
[null,"813 x 2032 x 44mm single exterior leaf solid core ","No.",7,"R                -","R                    -"]
[]
[null,"1200 x 2032 x 44mm single exterior leaf solid core ","No.",3,"R                -","R                    -"]
[]
[null,"FITTINGS"]
[]
[null,"The following in modular timber cupboards, counters, duty stations, desk etc. as per Cupboard Connections Specification"]
[null,"Carcasses of 16mm thick particle board with both faces white melamine with white Masonite backs. Shelving of 16mm particle board, both faces white melamine and front edge in white PVC. Doors of 16mm particle board with post formed vertical edges and laminated in Renolit. Tops of 32mm particle board with post formed leading edges and laminated in high pressure decorative laminate. All butt edges and edges against walls to be sealed with silicon sealant. Hinges to be “Hettich”. Drawer runners to be metal 500mm series with nylon runners or similar. All units complete with door, handles, hinges, cupboards, door, locks, barrel bolts and shelves. Floor unit complete with kick plates. (Formica tops measured elsewhere)   "]
[]
[null,"Built in cupboards fittings"]
[]
[null,"Kitchen sink floor cupboard 1200 x 600 x 900mm high with sides, bottom, back, 3 hinged doors and one drawer completely working including handles, etc. top and sink measured else where","No.",7,"R               -","R                    -"]
[]
[null,"Change room cabinet"]
[]
[null,"Locker to combines steel body with supawood beech veneer doors. Locker body to be epoxy coated and oven baked for superior finish with grey colour Standard body."]
[]
[null,"1800mm high x 450mm width x 500mm depth 2 door lockable lockers completely with heavy duty hinges and locks","No.",10,"R               -","R                    -"]
[]
[null,"COUNTER TOP"]
[]
[null,"Wrought hardwood to cupboards, etc"]
[]
[null,"19 x 70mm cleats","m",2,"R               -","R                    -"]
[]
[null,"19 x 50mm cleats fixed for worktop support ","m",2,"R               -","R                    -"]
[]
[null,"Interior type particle board with Formica veneer "]
[]
[null,"900 x30mm thick granite with all exposed edges large bevel edged, fixed to supports using dabs of 100% black silicone adhesive along all supports with all joints filled with matching polyester resin glue. Granite surface to be sealed using an approved stone sealer, all in accordance with the manufacturer's recommendations.","m",10,"R               -","R                    -"]
[]
[null,"2mm thick edge strip 32mm wide","m",25,"R               -","R                    -"]
[]
[null,"Interior type particle board with Formica veneer "]
[]
[null,"900 x30mm thick granite with all exposed edges large bevel edged, fixed to supports using dabs of 100% black silicone adhesive along all supports with all joints filled with matching polyester resin glue. Granite surface to be sealed using an approved stone sealer, all in accordance with the manufacturer's recommendations.","m",10,"R               -","R                    -"]
[]
[null,"2mm thick edge strip 32mm wide","m",25,"R               -","R                    -"]
[]
[null,"Cut 50mm work top to fit end bowl sink, measured else where ","No.",3,"R               -","R                    -"]
[]
[]
[null,"813 x 2032 x 44mm single leaf solid core with commercial veneer for paint.  pricing shall include painting as per manufactures specification"]
[]
[null,"G2 bullet resistant Anti-bandit door, complete with 100 x 50 x 3mm gauge mild steel rectangular frame and 25 x 25 x 3mm MS anlge rebates, overall size 930 x 2100mm high in paint finish with 250 X 500mm high BRG viewing panel glazed in 38mm thick bullet resistant glass with one-way vision film, supplied with a 6 pin tumbler key system, mortice dead lock with an additional heavy duty magnetic lock and striker including key switch and surface mounted casing, 6 Amp power supply, push buttons and interlock system, heavy duty aluminium continuous hinge, aluminium slam bar with heavy duty door closer and D-style pull handles. Door to comply to SABS 1658-1996"]
[]
[null,"Level G2 bullet resistant anti-badit internal door","No.",1,"R                -","R                           -"]
[]
[null,"Guard room"]
[]
[null,"Allow to supply and fit guard room window frame and bullet proof window pane, full measurements to ne verified on site.","m2",3,"R                -","R                           -"]
[]
[null,"BILL NO 5","Unit","QTY","Rate","Amount"]
[]
[null,"CEILING WORK"]
[]
[null,"SUPPLEMENTARY PREAMBLES "]
[]
[null,"Description "]
[]
[null,"Items described as “nailed” shall be deemed to be fixed with hardened steel nails or pins or shot pinned to brickwork or concrete"]
[]
[null,"Items described as “plugged” shall be deemed to include screwing to fibre, plastic or metal plugs at not exceeding 600mm centres, and where described as “bolted”, bolts priced elsewhere"]
[]
[null,"6.4mm “Rhino” gypsum plaster board with H-Type pressed steel jointing strips"]
[]
[null,"Ceiling including 38 x 38mm sawn softwood brandering at 450mm centres","m2",120,"R                -","R                    -"]
[]
[null,"Extra over ceiling for 800 x 800mm trap door of 38 50mm wrought softwood rebated framing with one 38 x 38mm sawn softwood cross brander covered with ceiling board and fitted flush in opening","No.",2,"R                -","R                    -"]
[]
[null,"“Rhino” gypsum plasterboard cornice"]
[]
[null,"75mm coved cornices","m2",120,"R                -","R                    -"]
[]
[null,"BILL NO 6","Unit","QTY","Rate","Amount"]
[]
[null,"IRONMONGERY"]
[]
[null,"LOCKS"]
[]
[null,"3 liver union lock with handles ","No.",12,"R               -","R                    -"]
[]
[null,"Ultra-security heavy duty locks","No.",13,"R               -","R                    -"]
[]
[null,"Stainless Steel Toilet Cubicle Indicator bolt & lock set, Grade 304Stainless Steel indicator bolt fixed to surface with matching stainless-steel screws.","No.",6,"R               -","R                    -"]
[]
[null,"Satin stainless-steel toilet roll holders for 2 rolls with central shaft system and cylinder lock, plugged and screwed to the wall with stainless steel screws. (vandal resistant)","No",6,"R                -","R                    -"]
[]
[]
[null,"SIGNAGE"]
[]
[null,"External signage"]
[]
[null,"500 x 150mm High double-sided ceiling mounted directional sign anodized aluminium female and male ablutions pictogram door sign, suspended from ceiling grids with brass chains. Minimum of 2,1m above finished floor level.","No.",2,"R               -","R                    -"]
[]
[null,"Allow to supply and fit station signage "]
[]
[null,"Station name, MLAMLANKUZI STATION to match the existing","No ",4,"R               -","R                    -"]
[]
[null,"BILL NO 7","Unit","QTY","Rate","Amount"]
[]
[null,"TILING"]
[]
[null,"Prices:"]
[]
[null,"Prices are to include for all square cutting and waste, cleaning off on completion and protection from injury. Areas are measured net to face of brickwork and concrete. Any additional area caused by the thickness of tiling and screed are to be allowed for in prices "]
[]
[null,"FLOOR TILING"]
[]
[null,"600x600mm Full Bodied polished Porcelain tiles with 3mm grouting lines"]
[]
[null,"On floors","m2",180,"R               -","R                    -"]
[]
[null,"300x300x6mm Full Bodied polished Porcelain mosaic tiles with 3mm grouting lines"]
[]
[null,"On floors","m2",180,"R               -","R                    -"]
[]
[null,"WALL TILING"]
[]
[null,"Matt Full Bodied Porcelain tiles, size 600 x 300mm x 12mm fixed to internal wall plaster backing with TAL tile adhesive mixed with TAL bonding liquid in lieu of water with joints continuous in both directions and grouted with TAL tile grout, excess grout on the surface to be cleaned with water as work proceeds."]
[]
[null,"On walls","m2",80,"R               -","R                    -"]
[]
[null,"300x300x6mm Full Bodied polished Porcelain mosaic tiles with 3mm grouting lines"]
[]
[null,"On walls","m2",80,"R               -","R                    -"]
[]
[]
[null,"BILL NO 8","Unit","QTY","Rate","Amount"]
[]
[null,"PLUMBING WORK "]
[]
[null,"SANITARY FITTINGS"]
[]
[null,"Vaal Sanitary ware Hibiscus vitreous china close coupled suite colour White , comprising 90º outlet open rim pan with matching 9 litre front single flush cistern including lid and fitments and Jazz Thermoset seat.","No.",9,"R                -","R                    -"]
[]
[null,"Vaal Sanitary ware Hibiscus vitreous china lavatory basin colour White, size 510 x 405mm with two tap hole including integrated overflow and chain stay hole bolted to wall with two x 10mm bolts and including Classic floor mounted pedestal and sealed with silicone sealant where basin meets wall.","No.",7,"R                -","R                    -"]
[]
[null,"Top entry ceramic urinal basin with Junior flush master exposed chrome flush valve including flush pipe, spreader, etc","No.",2,"R                -","R                    -"]
[]
[null,"WASTE UNINON ETC"]
[]
[null,"Bath and Basin waste, plug, chain, stay and backnut  ","No.",10,"R                -","R                    -"]
[]
[null,"TRAPS ETC"]
[]
[null,"365/40 CP bottle trap 40 x 40 INC CP/PVC adaptor to 40mm","No.",3,"R                -","R                    -"]
[]
[null,"38mm sink “P” trap","No.",9,"R                -","R                    -"]
[]
[null,"Brass shower P trap with square ss grating","No.",7,"R                -","R                    -"]
[]
[null,"SINK, BASIN, ETC"]
[]
[null,"90Mm Bsw 1200x500x180mm double bowl Kitchen stainless steel sink","No.",8,"R                -","R                    -"]
[]
[null,"TAPS, VALVES, ETC"]
[]
[null,"Kitchen sink Mixer taps","No.",8,"R                -","R                    -"]
[]
[null,"Push button pillar tap for hot and cold water","No.",18,"R                -","R                    -"]
[]
[null,"Flexi connector","No.",30,"R                -","R                    -"]
[]
[null,"15 Mini Ball Valve ","No.",30,"R                -","R                    -"]
[]
[null,"Single function vandal resistant shower head including shower arm, stainless steel polished body","No.",7,"R                -","R                    -"]
[]
[null,"Chrome plated Shower tap mixer","No.",7,"R                -","R                    -"]
[]
[null,"22mm Brass Gate Valve","No.",5,"R                -","R                    -"]
[]
[null,"600kpa pressure control valve","No.",3,"R                -","R                    -"]
[]
[null,"Relieve/safety valve","No.",6,"R                -","R                    -"]
[]
[null,"Vacuum breaker","No.",6,"R                -","R                    -"]
[]
[null,"Drain cock","No.",3,"R                -","R                    -"]
[]
[null,"0.8mm galvanized sheet iron"]
[]
[null,"125 x 100mm eaves gutter","m",50,"R                -","R                    -"]
[]
[null,"Extra over 125 x 100mm eaves gutter for stopped end","No.",8,"R                -","R                    -"]
[]
[null,"Extra over 125 x 100 eaves gutter for angle","No.",10,"R                -","R                    -"]
[]
[null,"Extra over 125 x 100mm eaves gutter for outlet for 100 x 75mm pipe","No.",10,"R                -","R                    -"]
[]
[null,"100 x 75mm rainwater pipes","m",25,"R                -","R                    -"]
[]
[null,"Extra over 100 x 75mm rainwater pipe for shoe","No.",10,"R                -","R                    -"]
[]
[null,"0.9mm galvanized sheet iron"]
[]
[null,"250 x 200mm industrial eaves gutter including heavy duty brackets fixed at 500mm centers","m",40,"R                -","R                    -"]
[]
[null,"Extra over 250 x 200mm eaves gutter for stopped end","No.",4,"R                -","R                    -"]
[]
[null,"Extra over 250 x 200 eaves gutter for angle","No.",6,"R                -","R                    -"]
[]
[null,"Extra over 125 x 100mm eaves gutter for outlet for 300mm pipe","No.",6,"R                -","R                    -"]
[]
[null,"300mm rainwater pipes","m",25,"R                -","R                    -"]
[]
[null,"Extra over 300mm rainwater pipe for shoe","No.",6,"R                -","R                    -"]
[]
[null,"Extra over PVC pipes for fittings"]
[]
[null,"110mm pan connector","No.",10,"R                -","R                    -"]
[]
[null,"WATER SUPPLIERS"]
[]
[null,"Class “O” copper pipe "]
[]
[null,"15mm pipes chased into brick walls","m",50,"R                -","R                    -"]
[]
[null,"22mm pipes","m",30,"R                -","R                    -"]
[]
[null,"22mm pipes chased into brick walls and make good","m",50,"R                -","R                    -"]
[]
[null,"Extra over class “O” copper pipes for capillary fittings"]
[]
[null,"15mm fitting  ","No.",15,"R                -","R                    -"]
[]
[null,"15mm Tee","No.",15,"R                -","R                    -"]
[]
[null,"15mm bend","No.",5,"R                -","R                    -"]
[]
[null,"22mm fitting  ","No.",20,"R                -","R                    -"]
[]
[null,"22mm Tee","No.",15,"R                -","R                    -"]
[]
[null,"22mm bend","No.",5,"R                -","R                    -"]
[]
[null,"ELECTRIC WATER HEATERS"]
[]
[null,"Supply, deliver and install Electrical geysers with all other accessories  "]
[null,"250L 600i dual electric water heater Geyser completely with safety valve, drain cock, vacuum breaker, gate valve, 1350 x 650mm tray and pressure regulating valve.","No.",2,"R                -","R                    -"]
[null,"25L 600i dual electric water heater Geyser completely with safety valve, drain cock, vacuum breaker","No ",6,"R                -","R                    -"]
[null,"Manhole covers and grid inlets"]
[]
[null,"560mm wide x 65mm thick heavy duty polymer grid inlet including frame","m",150,"R                -","R                    -"]
[]
[null,"SOIL DRAINAGE"]
[]
[null,"Upvc waste pipes"]
[]
[null,"50mm pipes with all connection and make good ","m",30,"R                -","R                    -"]
[]
[null,"Upvc class 34 pipes including excavation, bedding, backfilling and compaction and disposal of surplus material"]
[]
[null,"110mm pipes vertical or ramped to cleaning eyes etc (no excavation)","m",10,"R                -","R                           -"]
[]
[null,"110mm pipes laid in and including trenches not exceeding 1m deep","m",50,"R                -","R                           -"]
[]
[null,"50mm pipes with all connection and make good","m",5,"R                -","R                           -"]
[]
[null,"Extra over Upvc class 34 pipes for fittings"]
[]
[null,"110 Bend","No.",4,"R                -","R                           -"]
[]
[null,"110mm junction","No.",2,"R                -","R                           -"]
[]
[null,"110mm Access bend","No.",4,"R                -","R                           -"]
[]
[null,"Upvc Gulley"]
[null,"110mm Gulley not exceeding 1m deep formed of trap, vertical pipe and gully head with loose grating, encased in 15MPa unreinforced concrete, with top of gully 50mm above surrounding finished surfaces, top surface of concrete splayed and with 1:3 cement plaster on exposed surfaces","No.",2,"R                -","R                           -"]
[]
[null,"Sundries"]
[]
[null,"110mm Upvc cleaning eye to end of 110 Upvc pipe","No.",3,"R                -","R                           -"]
[]
[null,"350 x 350 x 50mm thick precast concrete inspection eye marker slab finished smooth on exposed surfaces with letters “I.E” or “I.O” on top and placed flush in ground or paving","No.",3,"R                -","R                           -"]
[]
[null,"Testing soil drainage system ","Item",null,"R                -","R                           -"]
[]
[null,"Manhole covers"]
[]
[null,"Precast concrete manholes with medium duty concrete manhole cover and frame bedded in 1:3 cement mortar, spacers bedded in 1:6 cement mortar and precast concrete slab including excavation, backfilling, compaction, risk of collapse, cartaway surplus material, 300mm thick unreinforced 20MPa/19mm concrete base projection75mm wide from walls, benching, junctions, channeling and step irons  "]
[]
[]
[null,"980mm diameter Precast concrete manhole cover including frame","No.",20,"R                -","R                           -"]
[]
[null,"Sewer connection"]
[]
[null,"Cutting into sides of existing manhole chamber for and connecting 110mm pipe including inserting 110mm channel junction and making good concrete benching","Item",null,"R                -","R                           -"]
[]
[null,"WATER RETICULATION"]
[]
[null,"PREMBLES"]
[]
[null,"The contractor is referred to the General Preambles for trades 2017 published by the Association of South Africa Quantity Surveyors before pricing"]
[]
[null,"WATER PIPEWORK"]
[]
[null,"HDPE PE 100PN 12.5 pipes including excavation, bedding, backfilling, and compaction and disposal of surplus material"]
[]
[null,"Fire hydrant system around the station building and platform",null,"Sum ","R                -","R                           -"]
[]
[]
[null,"Allow to supply and fit complete paraplegic toilet system including all necessary fittings and make good.",null,"Sum ","R                -","R                           -"]
[null,null,"Unit","QTY","Rate","Amount"]
[null,"BILL NO. 9"]
[]
[null,"GLAZING"]
[]
[null,"GLAZING TO ALUMINIUM WITH CLIP ON BEADS"]
[]
[null,"4mm patterned glass"]
[]
[null,"Panes exceeding 0.1m2 and 0.5 m2 ","m2",10,"R                -","R                    -"]
[]
[null,"4mm clear float glass"]
[]
[null,"Panes exceeding 0.1m2 and 0.5 m2 ","m2",5,"R                -","R                    -"]
[]
[null,"MIRROR"]
[]
[null,"6.5mm silvered float glass copper backed mirrors with polished adges holed for and fixed with chromium plated dome capped mirror screws with rubber buffers to plugs in brickwork "]
[]
[null,"Mirror 600 x 1200mm high with four screws ","No.",9,"R                -","R                    -"]
[]
[null,"Ticket window with window frame and bullet proof with prasa  full spec.","No ",3,"R                -","R                    -"]
[]
[null,"BILL NO.10","Unit","QTY","Rate","Amount"]
[]
[null,"METAL WORK"]
[]
[null,"PRESSED STEEL DOOR FRAMES, LOUVRE GRILLE FRAMES, ETC"]
[]
[null,"Preparation, supply and install 1.2mm Double rebated frames suitable for one brick work  "]
[]
[null,"External Frame for door 813 x 2032mm high","No.",5,"R                -","R                    -"]
[]
[null,"1.2mm Double rebated frames suitable for half brickwork  "]
[]
[null,"Internal Frame for door 813 x 2032mm high","No.",7,"R                -","R                    -"]
[]
[null,"SECURITY GATES "]
[]
[null,"Supply and install Burglar door"]
[]
[null,"815 x 2100mm high Heavy duty Burglar door and frame with 16mm steel round bar and 40 x 40 x 2.5mm square tubing as per attached drawing for single door","No.",5,"R                -","R                           -"]
[]
[null,"STEEL ROLLER SHUTTERS "]
[]
[null,"Roll-Up solid galvanised, SABS 1461, & epoxy coated M/S manually hand chain operated push-up roller shutter for maximum opening 3000 x 3000mm high with standard bottom rail, 75 x 0.8mm thick end-locked slats, 120mm extra-wide tamper proof guides, 4.5mm end plates, closed shaft and 2 x slidebolts, extruded with Aluminium Tbar & Astragal rubber weather seal. Including galv. cover box and powder coated components incl. door curtain, end plates, cover box, guides & T-bar. Door fixed to brick, concrete or structural steel jambs and concrete or steel lintel over. Contractor to provide cavity of 160mm x 120mm for recessing guides"]
[]
[null,"Manual hand chain Push-up Roller Shutters, for openings not exceeding 3000mm x 2500mm high.","No.",3,"R                -","R                           -"]
[]
[null,"Supply and install Burglar windows"]
[]
[null,"600mm W x 600mm H Box windows guard constructed with 5mm of expanded metal and 50 x 50 x 6mm equal angles. ","No.",8,"R                -","R                           -"]
[]
[null,"1200mm W x 600mm H Box windows guard constructed with 5mm of expanded metal and 50 x 50 x 6mm equal angles.","No.",4,"R                -","R                           -"]
[]
[null,"300mm W x 900mm H Box windows guard constructed with 5mm of expanded metal and 50 x 50 x 6mm equal angles.","No.",6,"R                -","R                           -"]
[]
[]
[null,"FENCING AND GATES"]
[]
[null,"CLEAR VIEW FENCING"]
[]
[null,"2500mm Panel Height, 2515mm Panel Width, 4.0mm Vertical Wire Dia, 3.15mm Horizontal"]
[null,"Wire Dia, 72x72x2mm Post Section, 2400mm Post Length, 4 Bends, 16 Clamps, 33.00kgs Panel Weight and 9.50kgs Upright weight"]
[]
[null,"Supply and erect 2.5 m high galvanized clear view fencing as per specification","m",800,"R                -","R                           -"]
[]
[null,"Supply and fit – replace heavy duty gate , with heavy duty industrial motor which allows to be operated manually also., allow all necessary fittings to be installed to the total completion of the job.",null,"Sum ","R               -","R                    -"]
[]
[null,"Replace the electric fence around the wall and allow for the new connection and allow to the full completion of job.",null,"Sum ","R               -","R                    -"]
[]
[null,"ALUMINIUM WINDOW FRAMES"]
[]
[null,"PT66 (600x600mm high) bronze window frame","No.",4,"R               -","R                    -"]
[]
[null,"PT126 (1200x600mm high) bronze window frame","No.",3,"R               -","R                    -"]
[]
[null,"PT159 (1500x900mm high) bronze window frame","No.",3,"R               -","R                    -"]
[]
[null,"Replace or redesign passenger shelters to match the existing and make good.","No ",4,"R               -","R                    -"]
[]
[null,"BILL NO.11","Unit","QTY","Rate","Amount"]
[]
[null,"PLASTERING"]
[]
[null,"SUPPLEMENTARY PREAMBLES "]
[]
[null,"Preparatory work for textured finishes:"]
[]
[null,"Textured finishes to be applied to plaster (plaster elsewhere )"]
[]
[null,"All surfaces are to be inspected and approved by Prasa representative before any work is commenced with "]
[]
[null,"Price for texture finishes:"]
[]
[null,"Prices are to include for all priming, preparatory work, etc"]
[]
[null,"INTERNAL PLASTER"]
[]
[null,"Preparation and Cement plaster on brick work"]
[]
[null,"walls ","m2",20,"R                -","R                    -"]
[]
[null,"Narrow width","m2",10,"R                -","R                    -"]
[]
[null,"BILL NO.12","Unit","QTY","Rate","Amount"]
[]
[null,"PAINTWORK"]
[]
[null,"For preambles see “Model Preambles for Trades” 2008 edition published by the Association of South African Quantity Surveyors "]
[]
[null,"SUPPLEMENTARY PREAMBLES"]
[]
[null,"Previously painted plastered surfaces "]
[]
[null,"Surfaces shall be thoroughly washed down and allowed to dry completely before any paint is applied. Blistered or peeling paint shall be completely removed and cracks shall be opened, filled with a suitable filler and finished smooth"]
[]
[null,"Previously painted metal surfaces "]
[null,"Surfaces shall be thoroughly rubbed and cleaned down. Blistered or peeling paint shall be completely removed down to bare metal"]
[]
[null,"Previously painted wood surfaces "]
[]
[null,"Surfaces shall be thoroughly cleaned down. Blistered or peeling paint shall be completely removed and cracks and crevices shall be primed, filled with a suitable filler and finished smooth"]
[]
[null,"PAINTWORK, ETC TO NEW WORK"]
[]
[null,"ON FLOATED PLASTER"]
[]
[null,"One coat professional plaster primer and two coats  acrylic paint "]
[]
[null,"On concrete sealing","m2",60,"R                -","R                    -"]
[]
[null,"One coat professional plaster primer and two coats contractors Brick and Slasto Dressing/Brick seal"]
[]
[null,"On internal and external face brick walls   ","m2",400,"R                -","R                           -"]
[]
[null,"Plastered walls ","m2",500,"R                -","R                           -"]
[]
[null,"ON WOOD"]
[]
[null,"One coat wood primer, one Universal Undercoat  and two coats PRASA Brown "]
[]
[null,"On Doors","No ",13,"R                -","R                           -"]
[]
[null,"ON METAL"]
[]
[null,"One coat zinc chromate primer, one Undercoat  and two coats Professional Gloss Enamel, including the steel structure"]
[]
[null,"One coat zinc chromate primer, one Undercoat  and two coats Chromadek Prasa Kingfisher Blue suitable for roof"]
[]
[null,"On roofs","m2",460,"R                -","R                           -"]
[]
[null,"One coat zinc chromate primer, one Undercoat  and two coats Chromadek Prasa Dove Grey suitable for roof"]
[]
[null,"On roofs","m2",200,"R                -","R                           -"]
[]
[null,"PAINTWORK, ETC TO PREVIOUSLY PAINTED  WORK"]
[]
[null,"Surface preparation and apply two coats acrylic paint "]
[]
[null,"On ceiling and cornices ","m2",100,"R                -","R                    -"]
[]
[null,"ON WOOD"]
[]
[null,"Surface preparation and apply two coats PRASA Brown "]
[]
[null,"On Doors","m2",50,"R                -","R                           -"]
[]
[null,"ON METAL"]
[]
[null,"One coat zinc chromate primer, one Undercoat  and two coats Professional Gloss Enamel"]
[]
[null,"On rails, bars, handrails, steel work, window frames, door frames, burglar gates and window, gates, gutters and down pipes","m2",50,"R                -","R                           -"]
[]
[]
[null,"Wash with polycell sugar soap and rinse with clean water to remove all traces of soap, remove all loose flaking paint and repair any cracks and defects, spot prime bare and repaired areas with bonding liquid and apply one coat sealer and two coats of interior quality nonconductive floor epoxy paint"]
[]
[null,"On floors","m2",200,"R                -","R                           -"]
[]
[null,"BILL NO. 13","Unit","QTY","Rate","Amount"]
[]
[null,"WATERPROOFING"]
[]
[null,"Waterproofing to roofs"]
[]
[null,"Preparation of surfaces including replacing of worn nails, Roll top ridging and corrugated roof sheeting","m2",120,"R                -","R                    -"]
[]
[null,"Polyester Membrane or any other approved with the applicable guarantee of five years Applied to bolt heads and lap joints applied as per manufactures specification and certificate of 5 year guarantee submitted after completion","m2",120,"R                -","R                    -"]
[]
[null,"WATERPROOFING TO ROOFS"]
[]
[null,"On flat concrete roofs slab with parapet walls"]
[]
[null,"Surface preparation, Supply and lay 4mm torch on waterproofing system saturated with Bitumen Silver UV protective agent (approved by the Professional Waterproofing Association) applied by means of the torch on fusion/gas weld application method, with 75mm overlaps, 100mm endlaps and 200mm upturns onto parapet walls. laid in strict accordance with Manufacturer's instructions","m2",80,"R                -","R                           -"]
[null,"BILL NO. 14","Unit","QTY","Rate","Amount"]
[]
[null,"BLINDS"]
[]
[null,"25mm aluminium venetian blinds including brackets and mounting accessories to fit 2000 x 1300mm high window opening","No.",4,"R                -","R                    -"]
[]
[null,"25mm aluminium venetian blinds including brackets and mounting accessories to fit 900 x 300mm high window opening","No.",4,"R                -","R                    -"]
[]
[null,"25mm aluminium venetian blinds including brackets and mounting accessories to fit 600 x 600mm high window opening","No.",4,"R                -","R                    -"]
[]
[null,"ELECTRICAL WORK"]
[]
[null,"SECTION 3"]
[null,"ELECTRICAL WORK"]
[]
[null,"Allow R1000 000.00 on Electrical Works and reticulation  to include all power supply to the station and connection from municipal supply to iclude but not limited to High mast pole street light fitting, The luminaire to consists of a separate lamp, control gear and spigot compartment. The control gear housing to be separated from the lamp housing for thermal reasons. To be designed to operate 70/400W mercury vapour and 70/400W high- pressure sodium/metal halide lamp. ",null,"SUM"]
{"$rows_empty":59}
[null," CONSTRUCTION COST"]
[]
[]
[null," FINAL SUMMARY"]
[null,"10 % Contingency fund"]
[]
[]
[]
[null,"SUB TOTAL"]
[]
[null,"ADD VAT @ 15%"]
[]
[null,"TOTAL AMOUNT "]

{"sheet":"NEW CANADA","index":7,"n_rows":661,"n_cols":6,"rows_kept":661,"merged":[[66,4,69,4],[66,5,69,5],[72,4,74,4],[72,5,74,5],[171,5,172,5],[379,2,380,2],[379,3,380,3],[379,4,380,4],[379,5,380,5],[435,1,436,1],[435,2,436,2],[435,3,436,3],[435,4,436,4],[435,5,436,5],[441,2,442,2],[441,3,442,3],[441,4,442,4],[441,5,442,5],[462,2,472,2],[462,3,472,3],[462,4,472,4],[462,5,472,5],[476,2,478,2],[476,3,478,3],[476,4,478,4],[476,5,478,5]],"flags":["formulas_cached_only"]}
[]
[null,"REFURBISHMENT OF NEW CANADA (Phase 1)- SOUTH GAUTENG REGION:RFQ NO: 13/07/2022/01CRES","Unit","Quantity","Rate","Amount"]
[]
["ITEM NO","SECTION 1"]
[null,"BILL NO. 1"]
[null,"PRELIMINARIES"]
[null,"BUILDING AGREEMENT AND PRELIMINARIES"]
[]
[null,"The JBCC Series 2000 Principal Building Agreement (July 2007"]
[null,"edition 5.0) prepared by the Joint Building Contracts"]
[null,"Committee, shall be the agreement, amended as hereinafter"]
[]
[null,"The Preliminaries for use with the JBCC Series 2000 Principal"]
[null,"Building Agreement (May 2005 edition) prepared by the Joint"]
[null,"Building Contracts Committee, shall be deemed to be"]
[null,"incorporated in these bills of quantities"]
[null,"Contractors are referred to the above-mentioned documents for"]
[null,"the full intent and meaning of each clause thereof"]
[null,"These clauses are hereinafter referred to by clause number"]
[null,"and heading only. Where standard clauses or alternatives are"]
[null,"not entirely applicable to this contract such modifications,"]
[null,"corrections or supplements as will apply are given under each"]
[null,"relevant clause heading and such modifications, corrections or"]
[null,"supplements shall take precedence notwithstanding anything"]
[null,"contrary contained in the above-mentioned documents"]
[]
[]
[null,"SECTION A: PRINCIPAL BUILDING"]
[null,"AGREEMENT"]
[null,"1 Clause 1.0 - Definitions and interpretation "]
[null,"Interpretation (A1-A7)"]
[]
[null,"SECTION B: GENERAL PRELIMINARIES"]
[]
[1,"1. General Preliminaries to Include Appointment of Local CLO ",{"$nulls":3},{"v":350000,"d":"R 350,000.00"}]
[]
[null,"SECTION NO. 2"]
[]
[null,"BILL NO. 1","Unit","QTY","Rate","Amount"]
[]
[null,"ALTERATIONS (PROVISIONAL)"]
[2]
[null,"REMOVAL OF EXISTING WORK"]
[]
[null,"Rove old steel gate  and deliver them at New canada depot 2km to and from site","no",4]
[3]
[null,"Remove old wire mesh fence 150m x 1.8  and deliver them at New canada depot 2km to and from site","no",1]
[]
[null,"FENCING CLEARE Vu"]
[]
[null,"Supply and instal sliding gate 3.2 x 2.1m Clear Vu gate","no ",1]
[]
[null,"Supply and install gate rail with6.5mx 15mm bar","no",1]
[]
[null,"Supply and install Clear Vu fence 140m x 2.1m in prasa blue colour","item ","Sum"]
[]
[null,"Supply and install Clear Vu  swing gate 1.2m x 2.1m in Prasa blue colour","item ","Sum"]
[]
[null,"GUARDROOM"]
[]
[null,"Replace poly vinile tile with polish Porseline ","m²",4]
[]
[null,"Supply and install electrical plug ","no",2]
[]
[null,"Supply and install floricent light complete with fitting","no",2]
[]
[null,"Replace external door ","no",1]
[]
[null,"Internal painting  ","m²",8]
[]
[null,"Monitor Room"]
[]
[null,"Re wire eletrical plugs ","no",6]
[]
[null,"Replace floricent lights complete with fittings ","no",12]
[]
[null,"Replace extractor fans ","no",4]
[]
[null,"Replace tile carpet ","m²",74]
[]
[null,"Paint internal walls with light grey paint","m²",200]
[]
[null,"Supply and tile potio","m²",4]
[]
[null,"Paint external walls with light grey paint","m²",260]
[]
[null,"Paint Ceiling white pva ","m²",110]
[]
[null,"Monitor Room Kitchen"]
[]
[null,"Replace steel cupboards with wood cupboards 4m x 600 mm","no",1]
[]
[null,"Supply and install cupboards bottom and top 3m x 600mm","no",1]
[]
[null,"Supply and install single ball sink ","no",1]
[]
[null,"Supply and install black grinite top 4m x 600 mm","no",1]
[]
[null,"Paint wall with light grey paint ","m²",35]
[]
[null,"Supply and install 10L hydroboiler","no",1]
[]
[null,"Supply and install external door ","no",1]
[]
[null,"Supply and install 100L Gyser","no",1]
[]
[null,"Monitor Room Bathroom"]
[]
[null,"Replace poly vinille with polish pocelean","m²",18]
[]
[null,"Replace floricent lights complete with fittings ","no",4]
[]
[null,"Replace extractor fan ","no",4]
[]
[null,"Public toilets"]
[]
[null,"External painting with light grey paint","m²",150]
[]
[null,"Paint gable end with light grey paint","m²",54]
[]
[null,"FENCE WALL PAINTING"]
[]
[null,"Paint fence wall internal and external with light grey paint","m2",7200]
[]
[null,"PLATFORM LIGHTING "]
[]
[null,"Replace faulty cable 6mm 4core cable ","m",25]
[]
[null,"Supply and install 32mm galvinised pipe sleeve ","m",6]
[]
[null,"Replace cercuit breakers 10 amps ","no",20]
[]
[null,"Wire for shelter lights 40m x 2.5mm cable ","no",20]
[]
[null,"Replace floricent lights complete with light fitting ","no",80]
[]
[null,"Replace high mass lights  ","no",48]
[]
[null,"GENERAL BUILDING "]
[]
[null,"Paint platform shelter with light grey paint","m²",2000]
[]
[null,"Paint platform shop with light grey paint ","m²",100]
[]
[null,"Waterproof shop roof slab ","m²",110]
[]
[null,"Paint roof slab over hang with light grey paint","m²",100]
[]
[null,"Demolish brick shelter wall ","m²",60]
[]
[null,"PLATFORM STAFF ROOM"]
[]
[null,"Supply and install 32mm HDP pipe","m",50]
[]
[null,"Supply and install 32mm gate valve ","no",2]
[]
[null,"Replace toilet pans ","no",2]
[]
[null,"Replace old sewer sv pipe ","m",6]
[]
[null,"Replace 110mm IE elbow sv","no",2]
[]
[null,"Replace 110mm T Junction sv","no",2]
[]
[null,"Replace handwash basin complete with basin mixer","no",2]
[]
[null,"Replace 15mm galvinised pipes with 15mm pax pipe ","m",25]
[]
[null,"Replace galvinised waste pipe with 50 mm sv pipe","m",6]
[]
[null,"Replace galvinised elbow with 50mm IE elbows","no",8]
[]
[null,"Supply and install single ball basin complete with zink mixer","no",1]
[]
[null,"Replace broken window panes 500 x 300","no",20]
[]
[null,"Supply and install external doors complete with locks","no",3]
[]
[null,"Supply and install standard burgler door ","no",1]
[]
[null,"Replace ceilling ","m²",24]
[]
[null,"Paint rhino boards with white pva paint ","m²",24]
[]
[null,"Paint internal wall with light grey paint","m²",88]
[]
[null,"Supply and install single plug","no",3]
[]
[null,"Supply and install light switch ","no",3]
[]
[null,"Supply and install min distribution box","no ",1]
[]
[null,"Supply and install 2m cupboards","no ",1]
[]
[null,"Supply and install single ball sink ","no",1]
[]
[null,"Supply and install 100L geyser","no",1]
[]
[null,"Supply and install 10L hydroboiler","no",1]
[]
[null,"Tile bathroom with 6 by 6 non slippery tile","m²",8]
[]
[null,"Tile over sink ","m²","1.2"]
[]
[null,"Rewire for 3 plugs and 5 lights","no",1]
[]
[null,"Supply and install domsetic lights ","no",5]
[]
[null,"Supply and install blinds 1.8 X 1.6","no",3]
[]
[null,"Supply and install Air corn ","no",1]
[]
[null,"PLATFORM STAFF ROOM"]
[]
[null,"Supply and install 32mm HDP pipe","m",50]
[]
[null,"Supply and install 32mm gate valve ","no",2]
[]
[]
[null,"Replace handwash basin complete with basin mixer","no",1]
[]
[null,"Replace 15mm galvinised pipes with 15mm pax pipe ","m",25]
[]
[null,"Replace galvinised waste pipe with 50 mm sv pipe","m",6]
[]
[null,"Replace galvinised elbow with 50mm IE elbows","no",8]
[]
[null,"Supply and install single ball basin complete with zink mixer","no",1]
[]
[null,"Replace ceilling ","m²",24]
[]
[null,"Paint rhino boards with white pva paint ","m²",24]
[]
[null,"Paint internal wall ","m²",88]
[]
[null,"Supply and install single plug","no",3]
[]
[null,"Supply and install light switch ","no",2]
[]
[null,"Supply and install min distribution box","no ",1]
[]
[null,"Supply and install 2m cupboards","no ",1]
[]
[null,"Supply and install single ball sink ","no",1]
[]
[null,"Supply and install 100L geyser","no",1]
[]
[null,"Supply and install 10L hydroboiler","no",1]
[]
[null,"Tile over sink ","m²","1.2"]
[]
[null,"Rewire for 3 plugs and 3 lights","no",1]
[]
[null,"Supply and install domsetic lights ","no",3]
[]
[null,"Supply and install blinds 1.8 X 1.6","no",2]
[]
[null,"Supply and install Air corn ","no",1]
[]
[null,"TOTAL CARRIED TO FINAL SUMMARY"]
[]
[]
[null,"SECTION No.1"]
[]
[null,"ALTERATION",null,"Bill No.1"]
[]
[null,"FENCING CLEAR Vu",null,"Bill No.2"]
[]
[null,"GUARD ROOM",null,"Bill No.3"]
[]
[null,"MONITOR ROOM",null,"Bill No.4"]
[]
[null,"PUBLIC TOILET",null,"Bill No.5"]
[]
[null,"FENCE WALL PAINTING ",null,"Bill No.6"]
[]
[null,"PLATFORM LIGHTING",null,"Bill No.7"]
[]
[null,"GENERAL BUILDING ",null,"Bill No.8"]
[]
[null,"PLATFORM STAFF ROOM",null,"Bill No.9"]
[]
[null,"FAULTY ROOM ",null,"Bill No.10"]
[]
[null," FINAL SUMMARY",{"$nulls":3},"R                    -"]
[]
[null,"10 % Contingency fund"]
[]
[null,"SUB TOTAL"]
[]
[null,"ADD VAT @ 15%"]
[]
[null,"TOTAL AMOUNT "]
{"$rows_empty":355}
[null," CONSTRUCTION COST"]
[]
[]
[null," FINAL SUMMARY"]
[null,"10 % Contingency fund"]
[]
[]
[]
[null,"SUB TOTAL"]
[]
[null,"ADD VAT @ 15%"]
[]
[null,"TOTAL AMOUNT "]