{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":329,"n_cols":7,"rows_kept":329,"merged":[[0,0,4,0],[0,1,4,1],[0,2,4,2],[0,5,4,5],[5,1,5,6],[21,0,21,3],[22,1,22,6],[40,0,40,3],[54,0,54,3],[70,1,70,4],[80,0,80,3],[83,0,83,1],[87,0,87,3],[93,0,93,3],[99,0,99,3],[104,0,104,3],[113,0,113,3],[119,0,119,3],[127,0,127,3],[133,0,133,3],[135,0,135,3],[140,0,140,3],[146,0,146,3],[150,0,150,3],[154,0,154,3],[159,0,159,3],[164,0,164,3],[169,0,169,3],[174,0,174,3],[179,0,179,3],[184,0,184,3],[189,0,189,3],[193,0,193,3],[194,0,199,0],[194,2,199,2],[194,3,199,3],[194,4,199,4],[194,5,199,5],[194,6,199,6],[204,0,204,3],[205,0,208,0],[205,2,208,2],[205,3,208,3],[205,4,208,4],[205,5,208,5],[205,6,208,6],[213,0,213,3],[214,0,217,0],[214,2,217,2],[214,3,217,3],[214,4,217,4],[214,5,217,5],[214,6,217,6],[222,0,222,3],[223,0,224,0],[229,0,229,3],[234,0,234,3],[241,0,241,3],[244,0,244,3],[246,0,246,3],[248,0,248,3],[250,0,250,3],[252,0,252,3],[254,0,254,3],[256,0,256,3],[258,0,258,3],[260,0,260,3],[262,0,262,3],[264,0,264,3],[266,0,266,3],[276,0,276,3],[287,0,287,3],[295,0,295,3],[301,0,301,3],[312,0,312,3],[327,0,327,3],[328,0,328,3]]}
["No","Description","Estimated Qty","Unit Rate","Total","15% VAT","Total"]
[]
[{"$nulls":4},"Unit Rate x EST QTY",null,"(Incl. 15% VAT)"]
[]
[{"$nulls":3},"(Excl. 15% VAT)","(Excl. 15% VAT)"]
[1,"D59 Welder’s 2 piece overalls as Specified"]
[1,"Sizes as follows:"]
[1.1,"34/30",29,"R","R","R","R"]
[1.2,"36/32",47,"R","R","R","R"]
[1.3,"38/34",60,"R","R","R","R"]
[1.4,"40/36",54,"R","R","R","R"]
[1.5,"42/38",73,"R","R","R","R"]
[1.6,"44/40",48,"R","R","R","R"]
[1.7,"46/42",41,"R","R","R","R"]
[1.8,"48/44",4,"R","R","R","R"]
[1.9,"50/46",4,"R","R","R","R"]
[1.1,"52/48",7,"R","R","R","R"]
[1.11,"54/50 ",2,"R","R","R","R"]
[1.12,"56/52",3,"R","R","R","R"]
[1.13,"58/54",2,"R","R","R","R"]
[1.14,"60/56",7,"R","R","R","R"]
["TOTAL FOR SECTION ",{"$nulls":3},"R","R","R"]
[2,"Conti suits, 2 piece acid resistant as specified"]
[null,"Sizes as follows;"]
[2.1,"28/24",4,"R","R","R","R"]
[2.2,"30/26",6,"R","R","R","R"]
[2.3,"32/28",14,"R","R","R","R"]
[2.4,"34/30",33,"R","R","R","R"]
[2.5,"36/32",60,"R","R","R","R"]
[2.6,"38/34",62,"R","R","R","R"]
[2.7,"40/36",39,"R","R","R","R"]
[2.8,"42/38",65,"R","R","R","R"]
[2.9,"44/40",31,"R","R","R","R"]
[2.1,"46/42",34,"R","R","R","R"]
[2.11,"48/44",6,"R","R","R","R"]
[2.12,"50/46",7,"R","R","R","R"]
[2.13,"52/48",4,"R","R","R","R"]
[2.14,"56/52",3,"R","R","R","R"]
[2.15,"58/54",1,"R","R","R","R"]
[2.16,"60/56",2,"R","R","R","R"]
["TOTAL FOR SECTION",{"$nulls":3},"R","R","R"]
[3,"DW-ARC15 (Navy Blue) 2-Piece collared long sleeve conti suit (Jacket and Pants) , with 50mm Silver flame retardant tape strips. as specified"]
[null,"Sizes as follows:"]
[3.1,"32/28",8,"R","R","R","R"]
[3.2,"34/30",15,"R","R","R","R"]
[3.3,"36/32",23,"R","R","R","R"]
[3.4,"38/34",38,"R","R","R","R"]
[3.5,"40/36",26,"R","R","R","R"]
[3.6,"42/38",23,"R","R","R","R"]
[3.7,"44/40",24,"R","R","R","R"]
[3.8,"46/42",9,"R","R","R","R"]
[3.9,"48/44",8,"R","R","R","R"]
[3.1,"50/48",3,"R","R","R","R"]
[3.11,"52/50",1,"R","R","R","R"]
["TOTAL FOR SECTION",{"$nulls":3},"R","R","R"]
[]
[4,"Rain suits yellow 2 piece virgin PVC high performance Heavy duty suit with printed 50mm silver reflective stripes on elbows and knees. SABS approved as specified"]
[null,"Sizes as follows:"]
[4.1,32,185,"R","R","R","R"]
[4.2,34,198,"R","R","R","R"]
[]
[5,"Reflective Bibs 100% polyester with a 25mm silver reflecting cross netted with JW logo and bindings on all ends as specified"]
[null,"Sizes as follows;"]
[5.1,"S",6,"R","R","R","R"]
[5.2,"M",53,"R","R","R","R"]
[5.3,"L",111,"R","R","R","R"]
[5.4,"XL",107,"R","R","R","R"]
[5.5,"XXL",38,"R","R","R","R"]
[5.6,"3XL",20,"R","R","R","R"]
[5.7,"4XL",20,"R","R","R","R"]
[null,"TOTAL FOR SECTION",{"$nulls":3},"R","R"]
[6,"Reflective Jacket (sleeveless) 100% polyester with a YKK zip front and I.D pocket, silver 50mm reflective tape and binding on all ends with JW Logo as specified"]
[null,"Sizes as follows;"]
[6.1,"S",101,"R","R","R","R"]
[6.2,"M",318,"R","R","R","R"]
[6.3,"L",366,"R","R","R","R"]
[6.4,"XL",237,"R","R","R","R"]
[6.5,"XXL",128,"R","R","R","R"]
[6.6,"3XL",76,"R","R","R","R"]
[6.7,"4XL",66,"R","R","R","R"]
["TOTAL FOR SECTION",{"$nulls":3},"R","R","R"]
[]
[7,"Aprons, for welders, chrome leather Grade A, long, heavy duty as specified"]
["Sizes 60 X 90cm"]
[7.1,"S",2,"R","R","R","R"]
[7.2,"M",2,"R","R","R","R"]
[7.3,"L",22,"R","R","R","R"]
["TOTAL FOR SECTION",{"$nulls":3},"R","R","R"]
[8,"Welders spats chrome leather Grade A ankle length heavy duty as specified"]
[]
[8.1,"S",3,"R","R","R","R"]
[8.2,"M",9,"R","R","R","R"]
[8.3,"L",64,"R","R","R","R"]
["TOTAL FOR SECTION",{"$nulls":3},"R","R","R"]
[9,"Welder spats chrome leather Grade A knee length heavy duty as specified"]
[null,"Sizes as follows;"]
[9.1,"S",3,"R","R","R","R"]
[9.2,"M",9,"R","R","R","R"]
[9.3,"L",14,"R","R","R","R"]
["TOTAL FOR SECTION",{"$nulls":3},"R","R","R"]
[10,"Welders yolkes chrome leather Grade A long sleeve heavy duty as specified"]
[null,"Sizes as follows;"]
[10.1,"M",3,"R","R","R","R"]
[10.2,"L",3,"R","R","R","R"]
["TOTAL FOR SECTION",{"$nulls":3},"R","R","R"]
[11,"Welders Leggings chrome leather Grade A heavy duty as specified"]
[null,"Sizes as follows;"]
[11.1,34,3,"R","R","R","R"]
[11.2,36,8,"R","R","R","R"]
[11.3,38,4,"R","R","R","R"]
[11.4,40,2,"R","R","R","R"]
[11.5,42,3,"R","R","R","R"]
[11.6,44,3,"R","R","R","R"]
["TOTAL FOR SECTION",{"$nulls":3},"R","R","R"]
[12,"Welders gauntlets chrome leather Grade A heavy duty.as specified"]
[null,"Sizes as follows;"]
[12.1,"S",3,"R","R","R","R"]
[12.2,"M",4,"R","R","R","R"]
[12.3,"L",9,"R","R","R","R"]
["TOTAL FOR SECTION",{"$nulls":3},"R","R","R"]
[13,"Welders chrome leather Grade A trousers heavy duty as specified"]
[null,"Sizes as follows;"]
[13.1,34,4,"R","R","R","R"]
[13.2,36,7,"R","R","R","R"]
[13.3,38,4,"R","R","R","R"]
[13.4,40,1,"R","R","R","R"]
[13.5,52,2,"R","R","R","R"]
["TOTAL FOR SECTION",{"$nulls":3},"R","R","R"]
[14,"Welders chrome leather Grade A jackets heavy duty as specified"]
[null,"Sizes as follows;"]
[14.1,"S",6,"R","R","R","R"]
[14.2,"M",6,"R","R","R","R"]
[14.3,"L",2,"R","R","R","R"]
["TOTAL FOR SECTION",{"$nulls":3},"R","R","R"]
[15,"Disposable Mop cap, white, non-woven. SABS approved products will take preference, where such approval exist. As Specified",45,"R","R","R","R"]
["TOTAL FOR SECTION",{"$nulls":3},"R","R","R"]
[16,"Gloves, Candy stripe pig skin working glove, Leather Palm Fabric (Candy) Back Glove. Pig split leather palm, thumb, back, knuckle, pull & tips. as specified"]
[16.1,"S",498,"R","R","R","R"]
[16.2,"M",597,"R","R","R","R"]
[16.3,"L",664,"R","R","R","R"]
["TOTAL FOR SECTION",{"$nulls":3},"R","R","R"]
[17,"Gloves, Cut and high resistant glove, Taeki5 or similar approved glove with a cut level of 5. as specified"]
[17.1,"S",900,"R","R","R","R"]
[17.2,"M",1158,"R","R","R","R"]
[17.3,"L",1256,"R","R","R","R"]
[17.4,"XL",862,"R","R","R","R"]
["TOTAL FOR SECTION",{"$nulls":3},"R","R","R"]
[18,"Gloves, green chrome leather, double padding on palm and finger area, 200mm cuffs heavy duty. as specified"]
[18.1,"M",3,"R","R","R","R"]
[18.2,"L",53,"R","R","R","R"]
["TOTAL FOR SECTION",{"$nulls":3},"R","R","R"]
[19,"Gloves, green chrome leather, double padding on palm and finger area, 400mm cuffs heavy duty. as specified"]
[19.1,"M",40,"R","R","R","R"]
[19.2,"L",53,"R","R","R","R"]
["TOTAL FOR SECTION",{"$nulls":3},"R","R","R"]
[20,"Gloves, PVC, lightweight, cotton flock inner lining, embossed grip finish, suppleness to allow freedom of hand movement, and waterproof, 200mm cuff heavy duty. as specified"]
[20.1,"S",100,"R","R","R","R"]
[20.2,"M",492,"R","R","R","R"]
[20.3,"L",508,"R","R","R","R"]
["TOTAL FOR SECTION",{"$nulls":3},"R","R","R"]
[21,"Gloves, PVC, lightweight, cotton flock inner lining, embossed grip finish, suppleness to allow freedom of hand movement, and waterproof, 400mm cuff heavy duty. as specified"]
[21.1,"S",100,"R","R","R","R"]
[21.2,"M",203,"R","R","R","R"]
[21.3,"L",253,"R","R","R","R"]
["TOTAL FOR SECTION",{"$nulls":3},"R","R","R"]
[22,"Gloves, PVC, lightweight, cotton flock inner lining, embossed grip finish, suppleness to allow freedom of hand movement, and waterproof, shoulder length heavy duty. as specified"]
[22.1,"S",50,"R","R","R","R"]
[22.2,"M",93,"R","R","R","R"]
[22.3,"L",103,"R","R","R","R"]
["TOTAL FOR SECTION",{"$nulls":3},"R","R","R"]
[23,"Gloves, PVC, lightweight, cotton flock inner lining, chip palm grip finish, suppleness to allow freedom of hand movement, and waterproof, 200mm cuff heavy duty. as specified"]
[23.1,"S",1100,"R","R","R","R"]
[23.2,"M",803,"R","R","R","R"]
[23.3,"L",853,"R","R","R","R"]
["TOTAL FOR SECTION",{"$nulls":3},"R","R","R"]
[24,"Gloves, PVC, lightweight, cotton flock inner lining, chip palm grip finish, suppleness to allow freedom of hand movement, and waterproof, 400mm cuff heavy duty. As Specified"]
[24.1,"S",1500,"R","R","R","R"]
[24.2,"M",401,"R","R","R","R"]
[24.3,"L",459,"R","R","R","R"]
["TOTAL FOR SECTION",{"$nulls":3},"R","R","R"]
[25,"Nitrile gloves, powder free. SABS approval or tested in accordance with the European directive for PPE (89/686/EEC) and tested to EN388 or EN407. As Specified"]
[25.1,"S",25,"R","R","R","R"]
[25.2,"M",1072,"R","R","R","R"]
[25.3,"L",1098,"R","R","R","R"]
["TOTAL FOR SECTION",{"$nulls":3},"R","R","R"]
[26,"Welder’s gloves blue cow split leather, lined with cotton padding, Yoke at the thumb, fingertips and hand stitching, 400mm cuffs heavy duty. As Specified"]
[null,"Sizes as follows;"]
[26.1,"M",10,"R","R","R","R"]
[26.2,"L",55,"R","R","R","R"]
["TOTAL FOR SECTION",{"$nulls":3},"R","R","R"]
[27,"Welder’s gloves blue cow split leather, lined with cotton padding. Yoke at the thumb, fingertips and had stitching, shoulder length heavy duty as specified."]
[null,"Sizes as follows;"]
[27.1,"L",20,"R","R","R","R"]
["TOTAL FOR SECTION",{"$nulls":3},"R","R","R"]
[28,"Elbow Length kitchen rubber gloves •Chemical resistance"]
[null,"• Airtight"]
[null,"• Elastic"]
[null,"• Made from C-type or CL-type rubber"]
[null,"• Extra-long arm length"]
[null,"• Suitable for working with acid in the laboratory"]
[null,"Sizes as follows:",null,"R","R","R","R"]
[28.1,"S",206,"R","R","R","R"]
[28.2,"M",342,"R","R","R","R"]
[28.3,"L",562,"R","R","R","R"]
["TOTAL FOR SECTION",{"$nulls":3},"R","R","R"]
[29,"Heat resistant gloves   "]
[null,"• Resist contact heat of up to 250°C"]
[null,"• Made from durable cowhide leather"]
[null,"• Non-Slippery finger tips"]
[29.1,"Sizes as follows:",null,"R","R","R","R"]
[29.2,"S",8,"R","R","R","R"]
[29.3,"M",23,"R","R","R","R"]
[29.4,"L",29,"R","R","R","R"]
["TOTAL FOR SECTION",{"$nulls":3},"R","R","R"]
[30,"Extra-long high temperature resistance glove  • Resist contact temperature of up to 500°C"]
[null,"• Made from Kevlar material"]
[null,"• Suitable for working with a furnace"]
[null,"• Elbow length arm protection"]
[null,"Sizes as follows:"]
[30.1,"S",6,"R","R","R","R"]
[30.2,"M",8,"R","R","R","R"]
[30.3,"L",6,"R","R","R","R"]
["TOTAL FOR SECTION",{"$nulls":3},"R","R","R"]
[31,"Household Bicolor Flocklined latex gloves"]
[null,"Sizes as follows"]
[31.1,"S",200,"R","R","R","R"]
[31.2,"M",512,"R","R","R","R"]
[31.3,"L",710,"R","R","R","R"]
[31.4,"XL",601,"R","R","R","R"]
["TOTAL FOR SECTION",{"$nulls":3},"R","R","R"]
[32,"Bicolor cotton lined latex gloves CE approved"]
[null,"Sizes as follows"]
[32.1,"M",150,"R","R","R","R"]
[32.3,"L",200,"R","R","R","R"]
[{"$nulls":4},"R","R","R"]
[33,"Extended cuff shoulder length PVC sewer gloves CE approved"]
[null,"Sizes as follows"]
[33.1,"S",50,"R","R","R","R"]
[33.2,"M",62,"R","R","R","R"]
[33.3,"L",98,"R","R","R","R"]
[33.4,"XL",50,"R","R","R","R"]
["TOTAL FOR SECTION",{"$nulls":3},"R","R","R"]
[]
[34,"Hard Hats light weight and comfortable high density polyethylene with fully adjustable headgear suspensions. as specified",1065,"R","R","R","R"]
["TOTAL FOR SECTION",{"$nulls":3},"R","R","R"]
[35,"Ear Plugs, QD30 or similar approved disposable, easy assembly, reusable ear plug with cord, flat noise attenuation, easy to lug and use, CI (Chief Inspector) number. as specified",2281,"R","R","R","R"]
["TOTAL FOR SECTION",{"$nulls":3},"R","R","R"]
[36,"Ear muffs, Noise reduction rating (NRR) of at least 26. To be supplied with instruction leaflet /manual, CI (Chief Inspector) number and SABS approved. as specified",575,"R","R","R","R"]
["TOTAL FOR SECTION",{"$nulls":3},"R","R","R"]
[37,"Spectacles, anti-chemical lens coating, light weight, soft nose pad. SABS approved products will take preference, where such approval exist as Specified",801,"R","R","R","R"]
["TOTAL FOR SECTION",{"$nulls":3},"R","R","R"]
[38,"Spectacles, light weight, anti-abrasive and anti-scratch. Angle of lens must be adjustable to at least three positions. Acceptable fit and comfort, impact resistant as specified",626,"R","R","R","R"]
["TOTAL FOR SECTION",{"$nulls":3},"R","R","R"]
[39,"Goggles, multi-purpose, soft PVC with indirect vents for use in a chemical environment, anti-fog acetate lens and must be capable of being worn with respirators as specified.",938,"R","R","R","R"]
["TOTAL FOR SECTION",{"$nulls":3},"R","R","R"]
[40,"Goggles, full face, clear lens, for use during grinding. SABS approved products will take preference, where such approval exist as Specified",186,"R","R","R","R"]
["TOTAL FOR SECTION",{"$nulls":3},"R","R","R"]
[41,"Welding Goggles, soft and comfortable. Must be capable of being worn over prescription glasses. ",166,"R","R","R","R"]
["TOTAL FOR SECTION",{"$nulls":3},"R","R","R"]
[42,"Welding Helmet, tough, robust and light weight. ",30,"R","R","R","R"]
["TOTAL FOR SECTION",{"$nulls":3},"R","R","R"]
[43,"Translight helmet for welders, self-adjusting. ",26,"R","R","R","R"]
["TOTAL FOR SECTION",{"$nulls":3},"R","R","R"]
[44,"Welder’ face shield. ",26,"R","R","R","R"]
["TOTAL FOR SECTION",{"$nulls":3},"R","R","R"]
[45,"Clear face shield chemical splash resistant with 1mm poly carbonate lens for laboratory use. ",75,"R","R","R","R"]
["TOTAL FOR SECTION",{"$nulls":3},"R","R","R"]
[46,"Dust Coats, khaki, 2 side pockets and a breast pocket with a silk-screened JW logo on left hand breast side and the City of Johannesburg logo silk-screened on the right breast side. As Specified"]
[null,"Sizes as follows:"]
[46.1,34,6,"R","R","R","R"]
[46.2,36,23,"R","R","R","R"]
[46.3,38,26,"R","R","R","R"]
[46.4,40,22,"R","R","R","R"]
[46.5,42,32,"R","R","R","R"]
[46.6,44,30,"R","R","R","R"]
[46.7,46,28,"R","R","R","R"]
["TOTAL FOR SECTION",{"$nulls":3},"R","R","R"]
[47,"Laboratory Coats, white, acid resistant, with press studs with a silk-screened JW logo on left hand breast side and the City of Johannesburg logo silk-screened on the right breast side. As Specified"]
[null,"Sizes as follows:"]
[47.1,34,8,"R","R","R","R"]
[47.2,36,6,"R","R","R","R"]
[47.3,38,4,"R","R","R","R"]
[47.4,40,4,"R","R","R","R"]
[47.5,42,3,"R","R","R","R"]
[47.6,44,4,"R","R","R","R"]
[47.7,46,2,"R","R","R","R"]
[47.8,48,4,"R","R","R","R"]
["TOTAL FOR SECTION",{"$nulls":3},"R","R","R"]
[48,"Laboratory Coats, navy blue, acid resistant, with press studs with a silk-screened JW logo on left hand breast side and the City of Johannesburg logo silk-screened on the right breast side. SABS approved products will take preference, where such approval exist. As Specified"]
[null,"Sizes as follows:"]
[48.1,34,5,"R","R","R","R"]
[48.2,36,20,"R","R","R","R"]
[48.3,38,20,"R","R","R","R"]
[48.4,40,10,"R","R","R","R"]
[48.5,42,10,"R","R","R","R"]
["TOTAL FOR SECTION",{"$nulls":3},"R","R","R"]
[49,"Acid resistant PVC white heavy duty apron, for laboratory use as specified"]
[]
[49.1,"S",8,"R","R","R","R"]
[49.2,"M",6,"R","R","R","R"]
[49.3,"L",6,"R","R","R","R"]
["TOTAL FOR SECTION",{"$nulls":3},"R","R","R"]
[]
[50,"Safety Durable white Bee Jackets with detachable Bee Veil Hood, Washable Bull Demin material Chest pocket and high-quality wrist bands. Products that have been assessed and certified by a SANAS accredited certification body to the relevant SANS specification will take preference and shall bear the certifications body’s mark of approval."]
[null,"Sizes as follows:"]
[50.1,"S",9,"R","R","R","R"]
[50.2,"M",15,"R","R","R","R"]
[50.3,"L",26,"R","R","R","R"]
[50.4,"XL",8,"R","R","R","R"]
[50.5,"2XL",23,"R","R","R","R"]
[50.6,"3XL",11,"R","R","R","R"]
[50.7,"4XL",5,"R","R","R","R"]
["TOTAL FOR SECTION",{"$nulls":3},"R","R","R"]
[51,"Rain Suits. The rains suits must be a yellow 2-piece high visibility polyester PVC with printed 50mm silver reflective stripes on elbows and ankles. Seams shall be reinforced and heat sealed for extra strength. The rain suit shall comprise of a stow away, clear side, panel hood with adjustable cord, concealed elastic cuff and draw cord in jacket hem with air vents under the arm and upper back. The trousers must include an elasticized waistband and ankle poppers on trouser hem. "]
[null,"Sizes as follows:"]
[51.1,36,236,"R","R","R","R"]
[51.2,38,171,"R","R","R","R"]
[51.3,40,97,"R","R","R","R"]
[51.4,42,63,"R","R","R","R"]
[51.5,44,61,"R","R","R","R"]
[51.6,46,35,"R","R","R","R"]
[51.7,48,34,"R","R","R","R"]
[51.8,50,10,"R","R","R","R"]
[51.9,52,12,"R","R","R","R"]
[52,54,6,"R","R","R","R"]
[52.1,56,10,"R","R","R","R"]
[52.2,60,6,"R","R","R","R"]
["TOTAL FOR SECTION",{"$nulls":3},"R","R","R"]
["GRAND TOTAL FOR ALL ITEMS OFFERED",{"$nulls":3},"R","R","R"]