{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Category A","Category B"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":6,"comments":4,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Category A","index":0,"n_rows":1216,"n_cols":18,"rows_kept":1216,"cut":false,"hidden":false,"merged":[]}
["C2.2 SCHEDULE OF RATES ","CATEGORY A - TERM TENDER FOR ROAD STRUCTURES AND ANCILLARY WORKS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["CHAPTER 1: GENERAL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["ITEM","DESCRIPTION","UNIT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["SECTION 1.2: GENERAL REQUIREMENTS AND PROVISIONS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.2.1","Environmental Management",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.2.1.1","Monitoring of compliance with and reporting on the EMP","day"]
["PSC1.2.1.3","Environmental Emergency Measures"]
["PSC1.2.1.3(a)","Provision of environmental emergency measures","PC Sum"]
["PSC1.2.1.3(b)","Contractor's charge to allow for handling costs and profit in respect of subitem PSC1.2.1.3(a) ","percentage (%)"]
["PSC1.2.1.4","Penalty to be deducted for non-compliance with requirements of Environmental management"]
["PSC1.2.1.4(a)","Vehicles, plant or materials related to the Contractor’s operations, parked or stored outside the demarcated boundaries of the Site","Number (No)"]
["PSC1.2.1.4(b)","Persons, vehicles, plant or materials related to the Contractor’s operations, found within the designated boundaries of a “no go” area","Number (No)"]
["PSC1.2.1.4 (c)","Persistent and unrepaired oil leaks from machinery/not using a drip tray to collect waste oil and other lubricants/not using specified absorbent material to encapsulate hydrocarbon spillage/using inappropriate methods of refuelling (the use of a funnel rather than a pump). ","Number (No)"]
["PSC1.2.1.4 (d)","Refuelling in areas not approved by the Employer’s Agent. ","Number (No)"]
["PSC1.2.1.4(e)","Waste and Litter on Site.","Number (No)"]
["PSC1.2.1.4(f)","Deliberate lighting of fires on Site.  ","Number (No)"]
["PSC1.2.1.4(g)","Individual not making use of the Site ablution facilities. ","Number (No)"]
["PSC1.2.1.4(h)","Damage to trees not specified to be removed. ","Number (No)"]
["PSC1.2.1.4(i)","Dust or excessive noise emanating from the site ","Number (No)"]
["PSC1.2.1.4 (j)","Damage or pollution of wetlands, rivers and surrounding areas","Number (No)"]
["PSC1.2.2","Programming and Reporting"]
["PSC1.2.2.1","Submission of a Scheme 1 Programme","lump sum"]
["PSC1.2.4","Stakeholder liaison"]
["PSC1.2.4.1","Remuneration of Community Liaison Officer (CLO) (as per CCT published rate. CPA will apply if rate is revised)                         ","day"]
["PSC1.2.4.2","Contractor’s charge to allow for handling costs and profit in respect of subitem PSC1.2.4.1            ","percentage (%)"]
["PSC1.2.5","Safety "]
["C1.2.5.1","Health and safety plan","lump sum"]
["PSC1.2.5.2","Implementation of health and safety plan","day"]
["PSC1.2.8","Dayworks"]
["PSC1.2.8.1","Personnel"]
["PSC1.2.8.1(a)","Unskilled labourer","hour (h)"]
["PSC1.2.8.1(b)","Semi-skilled labourer","hour (h)"]
["PSC1.2.8.1(c)","Skilled labourer","hour (h)"]
["PSC1.2.8.1(d)","Gang leader","hour (h)"]
["PSC1.2.8.1(e)","Foreman","hour (h)"]
["PSC1.2.8.1(f)","Skilled artisan","hour (h)"]
["PSC1.2.8.1(g)","Welder (in accordance with welder qualification requirements of A13.11.8.1(b))","hour (h)"]
["PSC1.2.8.2","Construction equipment"]
["PSC1.2.8.2(a)","Tractor loader backhoe (55kW)","hour (h)"]
["PSC1.2.8.2(b)","Generator","hour (h)"]
["PSC1.2.8.2(c)","Compressor","hour (h)"]
["PSC1.2.8.2(d)","Welding machine (500A)","hour (h)"]
["PSC1.2.8.2(e)","Other Plant/Equipment not specified above"]
["PSC1.2.8.2(e)(i)","Procurement of plant/equipment- actual cost of plant/equipment not already specified in the tender by the employer","provisional sum"]
["PSC1.2.8.2(e)(ii)","Handling cost, profit and all other charges in respect of item PSC1.2.8.2(h)(i)","percentage (%)"]
["C1.2.8.3","Vehicles "]
["C1.2.8.3(a)","Light delivery vehicle (1 tonne)","kilometre (km)"]
["C1.2.8.3(b)","Flatbed truck (with crane capable of transporting and placing/removing concrete new jersey type barriers)","kilometre (km)"]
["C1.2.8.3(c)","Dump truck (6m³)","kilometre (km)"]
["C1.2.8.4","Materials"]
["C1.2.8.4(a)","Procurement of materials","provisional sum"]
["C1.2.8.4(b)","Contractor's handling costs, profit and all other charges in respect of item C1.2.8.4(a)","percentage (%)"]
["PSC1.2.10","Dispute Adjudication Board (DAB)"]
["PSC1.2.10.1","Employer’s contribution to DAB (50%)","PC Sum"]
["CHAPTER 1: GENERAL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["ITEM","DESCRIPTION","UNIT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["SECTION 1.3: CONTRACTOR’S ESTABLISHMENT ON SITE AND GENERAL OBLIGATIONS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.3.1","The Contractor's general obligations",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.3.1.1","The Contractor’s general obligations for Work Projects greater than R1 000 001 up to and including R1 500 000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.3.1.1(a)","Fixed obligations","lump sum",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.3.1.1(b)","Time-related obligations","day",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.3.1.1(c)","Extra-over sub-items (a) and (b) for working on designated non-working and special non-working days as instructed by the Employer","day",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.3.1.2","The Contractor’s general obligations for Work Projects greater than R1 500 001 up to and including R2 000 000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.3.1.2(a)","Fixed obligations","lump sum",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.3.1.2(b)","Time-related obligations","day",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.3.1.2(c)","Extra-over sub-items (a) and (b) for working on designated non-working and special non-working days as instructed by the Employer","day",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.3.1.3","The Contractor’s general obligations for Work Projects greater than R2 000 001 up to and including R2 500 000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.3.1.3(a)","Fixed obligations","lump sum",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.3.1.3(b)","Time-related obligations","day",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.3.1.3(c)","Extra-over sub-items (a) and (b) for working on designated non-working and special non-working days as instructed by the Employer","day",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.3.1.4","The Contractor’s general obligations for Work Projects greater than R2 500 001 up to and including R3 000 000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.3.1.4(a)","Fixed obligations","lump sum",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.3.1.4(b)","Time-related obligations","day",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.3.1.4(c)","Extra-over sub-items (a) and (b) for working on designated non-working and special non-working days as instructed by the Employer","day",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.3.2","Contract sign boards","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["CHAPTER 1: GENERAL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["ITEM","DESCRIPTION","UNIT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["SECTION 1.5: ACCOMMODATION OF TRAFFIC",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.5.1","Accommodation of pedestrian and non-motorised traffic",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.5.1.1","Accommodation of pedestrian and non-motorised traffic","day",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.5.2","Accommodation of vehicular traffic",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.5.2.1","Class 1: principal arterial (40 000 < vpd < 120 000)","day",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.5.2.2","Class 2: major arterial (20 000 < vpd < 60 000)","day",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.5.2.3","Class 3: minor arterial (10 000 < vpd < 40 000)","day",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.5.2.4","Class 4a: collector street, commercial (vpd < 25 000)","day",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.5.2.5","Class 4b: collector street, residential (vpd < 15 000)","day",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.5.2.6","Class 5a: local street, commercial (vpd < 5 000)","day",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.5.7","Temporary traffic control facilities",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5.7.1","Delineators including mounting bases and ballast:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5.7.1(a)","Single sided, reversible left or right (200 x 800mm)","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5.7.1(b)","Double sided, reversible left or right (200 x 800mm)","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5.7.2","Traffic cones, minimum height 750mm","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5.7.3","Flagmen","man-shift",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5.7.4","Traffic controllers","man-shift",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5.7.5","Provision of illuminated traffic signs:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5.7.5(a)","Sign mounted flashing amber lights (2 lights with the specified power supply) \nmounted on abacking board which is:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5.7.5(a)(i)","900mm wide x 150mm high","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5.7.5(a)(ii)","1200mm wide x 200mm high","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5.7.5(b)","Flashing LED illuminated arrow board","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.5.7.8","Traffic control stations","day",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.5.7.9","Cleaning of traffic control facilities","day",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.5.7.10","Barriers manufactured from plastic and ballasted with sand or water","metre (m)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.5.8","Traffic safety officer","man-shift",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.5.9","Traffic safety vehicle","day",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5.12","Additional traffic accommodation facilities ordered by the Engineer:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5.12.1","Provision of additional traffic accommodation facilities ","provisional sum",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5.12.2","Handling cost, profit and all other charges in respect of item C1.5.12.1","percentage (%)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.5.13","Penalty to be deducted for non-compliance with requirements for accommodation of traffic",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.5.13.1","Fixed penalty per occurrence","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.5.13.2","Time-related penalty","hour (hr)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5 / C11.4.2","Performance based vehicle restraint systems",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5/C11.4.2.1","Complete longitudinal barrier system to EN 1317 or AASHTO MASH or NCHRP350 as alternative where no MASH product is available:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5/11.4.2.1(c)","Concrete barrier system (H1, W4 according to EN1317 or MASH equivalent)","metre (m)"]
["C1.5/11.4.2.2","Terminal sections for the following to EN 1317 or AASHTO MASH or NCHRP350 as alternative where no MASH product is available:"]
["C1.5/11.4.2.2(a)","End treatments (Test Level 80/1 according to EN1317-3 or MASH equivalent)","number (No.)"]
["C1.5/11.4.2.3","Relocation of temporary systems (H1, W4 according to EN1317 or MASH equivalent)","metre (m)"]
["C1.5/C11.6.1.8","Regulatory signs, temporary (TR-series)"]
["C1.5/C11.6.1.8(a)","600mm size ","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5/C11.6.1.8(b)","900mm size ","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5/C11.6.1.8(c)","1200mm size ","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5/C11.6.1.10","Warning signs, temporary (TW-series) ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5/C11.6.1.10(a)","600mm size ","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5/C11.6.1.10(b)","900mm size ","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5/C11.6.1.10(c)","1200mm size ","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5/C11.6.1.10(d)","1500mm size ","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5/PSC11.6.1.13","Portable STOP and GO-RY signs","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5/PSC11.6.1.14","Other temporary standard road signs not specified above (STW-/DTG-/TGS-/TG-/TIN-series)","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["CHAPTER 1: GENERAL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["ITEM","DESCRIPTION","UNIT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["SECTION 1.6: CLEARING AND GRUBBING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.6.1","Clearing"]
["PSC1.6.1.1","Clearing with machines and some hand labour where necessary","square metre (m2)"]
["PSC1.6.1.2","Clearing with hand labour only when labour enhanced work is specified","square metre (m2)"]
["PSC1.6.2","Grubbing"]
["PSC1.6.2.1","Grubbing with machines and some hand labour where necessary","square metre (m2)"]
["PSC1.6.2.2","Grubbing with hand labour when labour enhancement work is specified or it is not practical to use a machine","square metre (m2)"]
["C1.6.3","Removal and grubbing of large trees and tree stumps:"]
["C1.6.3.1","Girth equal to or exceeding 1,0m up to and including 2,0m","number (No.)"]
["C1.6.3.2","Girth exceeding 2,0m up to and including 3,0m","number (No.)"]
["C1.6.3.3","Girth exceeding 3,0m","number (No.)"]
["CHAPTER 1: GENERAL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["ITEM","DESCRIPTION","UNIT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["SECTION 1.7: LOADING AND HAULING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.7.2","Hauling"]
["C1.7.2.2","Hauling material to spoil and off-loading it at a designated spoil or stockpile area:"]
["C1.7.2.2(a)","Cleared and grubbed material (organic matter and all other unsuitable or waste material)","cubic metre kilometre (m3.km)"]
["C1.7.2.2(b)","Soil and gravel material","cubic metre kilometre (m3.km)"]
["C1.7.2.2(c)","Boulders, hard material and concrete","cubic metre kilometre (m3.km)"]
["CHAPTER 2: SERVICES",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["ITEM","DESCRIPTION","UNIT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["SECTION 2.1: GENERAL REQUIREMENTS AND TRENCHING FOR SERVICES",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C2.1.1","Location, identification, protection and relocation of existing services"]
["C2.1.1.2","Permanent services relocation or protection work by others","PC Sum"]
["C2.1.1.3","Handling costs and profit in respect of item C2.1.1.2 above","percentage (%)"]
["CHAPTER 3: DRAINAGE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["ITEM","DESCRIPTION","UNIT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["SECTION 3.1: DRAINS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C3.1.2","Clearing, shaping and disposal of accumulated sediment in existing unlined open drains "]
["C3.1.2.1","Using conventional methods","cubic metre (m3)"]
["C3.1.2.2","Using labour enhanced construction methods","cubic metre (m3)"]
["C3.1.3","Excavation, clearing and disposal of accumulated sediment in existing lined drains and drainage systems"]
["C3.1.3.1","Using conventional methods (up to 1,5m):"]
["C3.1.3.1(a)","Manholes and inlet and outlet structures","cubic metre (m3)"]
["C3.1.3.1(b)","Culvert barrels","cubic metre (m3)"]
["C3.1.3.1(c)","Concrete or other lined side drains","cubic metre (m3)"]
["C3.1.3.2","Using conventional methods (in excess of 1,5m):"]
["C3.1.3.2(a)","Manholes and inlet and outlet structures","cubic metre (m3)"]
["C3.1.3.2(b)","Culvert barrels","cubic metre (m3)"]
["C3.1.3.2(c)","Concrete or other lined side drains","cubic metre (m3)"]
["C3.1.3.3","Using labour enhanced construction methods:"]
["C3.1.3.3(a)","Manholes and inlet and outlet structures","cubic metre (m3)"]
["C3.1.3.3(b)","Culvert barrels","cubic metre (m3)"]
["C3.1.3.3(c)","Concrete or other lined side drains","cubic metre (m3)"]
[]
["CHAPTER 3: DRAINAGE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["ITEM","DESCRIPTION","UNIT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["SECTION 3.3: CONCRETE KERBING AND CHANNELING, ASPHALT BERMS, CHUTES, DOWNPIPES, AS WELL AS CONCRETE, STONE PITCHED AND GABION LININGS FOR OPEN DRAINS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC3.3.1","Concrete kerbing:"]
["C3.3.1.1","Prefabricated kerbing"]
["C3.3.1.1(a)","E3 Edging (see Drawing No. RD1.3)"]
["C3.3.1.1(a)(i)","300mm units","metre (m)"]
["C3.3.1.1(a)(ii)","1000mm units","metre (m)"]
["C3.3.1.1(b)","E1 Edging (see Drawing No. RD1.3)"]
["C3.3.1.1(b)(i)","300mm units","metre (m)"]
["C3.3.1.1(b)(ii)","1000mm units","metre (m)"]
["C3.3.1.2","Cast in situ kerbing "]
["C3.3.1.2(a)","Transition kerb (BK2 to MK10) (RD1.1 to RD1.2)"]
["C3.3.1.2(a)(i)","1000mm units","metre (m)"]
["PSC3.3.1.3","Concrete channelling:"]
["PSC3.3.1.3(a)","Precast half round channel (see Drawing No. RD1.7)"]
["PSC3.3.1.3(a)(i)","Type W1","metre (m)"]
["PSC3.3.1.3(a)(ii)","Type W2","metre (m)"]
["PSC3.3.1.3(a)(iii)","Type W3","metre (m)"]
["PSC3.3.1.3(b)","Triple flat channel (2 No x C1 Channels plus 1 No C2 channel) (See drawing No RD1.4)","metre (m)"]
["PSC3.3.1.4","Extra over for item PSC3.3.1.3(b), for in-situ Concrete infill "]
["PSC3.3.1.4(a)","Cast in-situ 50mm width","metre (m)"]
["PSC3.3.1.4(b)","Cast in-situ 75mm width","metre (m)"]
["PSC3.3.1.4(c)","Cast in-situ 100mm width","metre (m)"]
["C3.3.5","Asphalt berms"]
["C3.3.5.1","Asphalt berms placed where there are no vehicle restraint systems (refer to dwg RD13.2) ","metre (m)"]
["C3.3.5.2","Asphalt berms placed at existing vehicle restraint systems  (refer to dwg RD13.2) ","metre (m)"]
["C3.3.5.4","Bond coat (30% stable grade emulsion)","square metre (m2)"]
["C3.3.10","Sealed joints in concrete and stone pitched linings of open drains "]
["C3.3.10.1","Silicone sealant (up to 10mm wide, including a closed cell polyethylene backing rope; Silicone sealant to be in accordance with Clause A6.1.5.7c and applied in accordance with the manufacturer's instructions)","metre (m)"]
["C3.3.11","Concrete screed or backfill below chutes (15 MPa concrete)","cubic metre (m3)"]
["C3.3.13","Polymer film sheeting (375 Micron) for concrete-lined open drains","square metre (m2)"]
["C3.3.14","Cutting bituminous surfacing and pavement layers for concrete kerbing, channelling or concrete-lined drains","metre (m)"]
["C3.3.15","Energy dissipaters in outlet structures"]
["C3.3.15.2","Stones set in outlet structures","square metre (m2)"]
["PSC3.3.16","Demolition and removal of existing kerbs and/or channel","cubic metre (m3)"]
["PSC3.3.17","Remove existing kerbing, channelling and edging and set aside for reuse"]
["PSC3.3.17(a)","Precast kerb","metre (m)"]
["PSC3.3.17(b)","Precast channel"]
["PSC3.3.17(b)(i)","Single ","metre (m)"]
["PSC3.3.17(b)(ii)","Double","metre (m)"]
["PSC3.3.17(b)(iii)","Triple","metre (m)"]
["PSC3.3.17(c)","Precast kerb and channel","metre (m)"]
["PSC3.3.17(d)","Precast edging","metre (m)"]
["PSC3.3.17(e)","Extra-over for item PSC3.3.17(a)-(d) for removing granite kerbing, channelling and edging","metre (m)"]
["PSC3.3.18","Relay existing concrete kerbing and/or channelling and edging"]
["PSC3.3.18(a)","Precast kerb only","metre (m)"]
["PSC3.3.18(b)","Precast channel only"]
["PSC3.3.18(b)(i)","Single ","metre (m)"]
["PSC3.3.18(b)(ii)","Double","metre (m)"]
["PSC3.3.18(b)(iii)","Triple","metre (m)"]
["PSC3.3.18(c)","Precast kerb and channel","metre (m)"]
["PSC3.3.18(d)","Precast edging - Type E3","metre (m)"]
["PSC3.3.18(e)","Precast edging - Type E1","metre (m)"]
["PSC3.3.18(f)","Extra-over for item PSC3.3.18(a)-(e) for relaying granite kerbing, channelling and edging","metre (m)"]
["PSC3.3.19","Special backfilling of kerbs using:"]
["PSC3.3.19(a)","G5 quality material from commercial sources","cubic metre (m3)"]
["PSC3.3.19(b)","Reclaimed Asphalt from site","cubic metre (m3)"]
["PSC3.3.19(c)","Reclaimed asphalt from depot, including loading and free-haul up to 5km","cubic metre (m3)"]
["PSC3.3.20","New concrete chutes or repair of existing concrete chutes","cubic metre (m3)"]
["CHAPTER 8: REPAIR EXISTING LAYERS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["ITEM","DESCRIPTION","UNIT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["SECTION 8.8: PATCHING AND EDGE BREAK REPAIR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C8.8.1","Saw cutting pavement layers for patching"]
["C8.8.1.1","Asphalt or bituminous surfacing to an average depth"]
["C8.8.1.1(a)","Not exceeding 50mm","metre (m)"]
["C8.8.1.1(b)","Exceeding 50mm but not exceeding 100mm","metre (m)"]
["C8.8.1.1(c)","Exceeding 100mm","metre (m)"]
["C8.8.1.2","Cemented pavement layers to an average depth"]
["C8.8.1.2(a)","Not exceeding 100mm","metre (m)"]
["C8.8.1.2(b)","Exceeding 100mm but not exceeding 200mm","metre (m)"]
["C8.8.1.2(c)","Exceeding 200mm","metre (m)"]
["C8.8.1.3","Granular layers to an average depth"]
["C8.8.1.3(a)","Not exceeding 100mm","metre (m)"]
["C8.8.1.3(b)","Not exceeding 200mm","metre (m)"]
["C8.8.1.3(c)","Exceeding 200mm","metre (m)"]
["C8.8.2","Excavation in existing pavements for patching (non-milling)"]
["C8.8.2.1","Asphalt layers"]
["C8.8.2.1(a)","Not exceeding 10 m² including for edge repairs wider than 250mm","cubic metre (m3)"]
["C8.8.2.1(b)","Exceeding 10 m² but not exceeding 50 m² including for edge repairs wider than 250mm","cubic metre (m3)"]
["C8.8.2.1(c)","Exceeding 50 m² up to 100 m² including for edge repairs wider than 250mm","cubic metre (m3)"]
["C8.8.2.1(d)","Exceeding 100 m²","cubic metre (m3)"]
["C8.8.2.2","Cemented layers"]
["C8.8.2.2(a)","Not exceeding 10 m² including for edge repairs wider than 250mm","cubic metre (m3)"]
["C8.8.2.2(b)","Exceeding 10 m² but not exceeding 50 m² including for edge repairs wider than 250mm ","cubic metre (m3)"]
["C8.8.2.2(c)","Exceeding 50 m² up to 100 m² including for edge repairs wider than 250mm","cubic metre (m3)"]
["C8.8.2.2(d)","Exceeding 100 m²","cubic metre (m3)"]
["C8.8.2.3","Other layers (granular layers)"]
["C8.8.2.3(a)","Not exceeding 10 m² including for edge repairs wider than 250mm","cubic metre (m3)"]
["C8.8.2.3(b)","Exceeding 10 m² but not exceeding 50 m² including for edge repairs wider than 250mm","cubic metre (m3)"]
["C8.8.2.3(c)","Exceeding 50 m² up to 100 m² including for edge repairs wider than 250mm","cubic metre (m3)"]
["C8.8.2.3(d)","Exceeding 100 m²","cubic metre (m3)"]
["C8.8.3","Compacting the floor of excavations for patching (compacted in 150mm layers and to 100% of maximum dry density for sand and 97% of maximum dry density for gravel)","square metre (m2)"]
["PSC8.8.4","Backfilling of excavations for patching with:"]
["PSC8.8.4.3","Asphalt"]
["PSC8.8.4.3(a)","Continuously graded (sand skeletal) using a PG58V-22 (A-E2) binder with a surface area:"]
["PSC8.8.4.3(a)(i)","Not exceeding 10 m² including for edge repairs wider than 250mm","ton (t)"]
["PSC8.8.4.3(a)(ii)","Exceeding 10 m² but not exceeding 50 m² including for edge repairs wider than 250mm","ton (t)"]
["PSC8.8.4.3(a)(iii)","Exceeding 50 m² up to 100 m² including for edge repairs wider than 250mm","ton (t)"]
["PSC8.8.4.3(a)(iv)","Exceeding 100 m²","ton (t)"]
["PSC8.8.4.3(b)","Cold-mix asphalt: certified by Agrèment SA as a minimum of Class 2 type with a surface area:"]
["PSC8.8.4.3(b)(i)","Not exceeding 10 m² including for edge repairs wider than 250mm","ton (t)"]
["PSC8.8.4.3(b)(ii)","Exceeding 10 m² but not exceeding 50 m² including for edge repairs wider than 250mm","ton (t)"]
["PSC8.8.4.3(b)(iii)","Exceeding 50 m² up to 100 m² including for edge repairs wider than 250mm","ton (t)"]
["PSC8.8.4.3(b)(iv)","Exceeding 100 m²","ton (t)"]
["C8.8.4.4","Granular base material (G4) for a patch with a surface area"]
["C8.8.4.4(a)","Not exceeding 10 m² including for edge repairs wider than 250mm","ton (t)"]
["C8.8.4.4(b)","Exceeding 10 m² but not exceeding 50 m² including for edge repairs wider than 250mm","ton (t)"]
["C8.8.4.4(c)","Exceeding 50 m² up to 100 m² including for edge repairs wider than 250mm","ton (t)"]
["C8.8.4.4(d)","Exceeding 100 m²","ton (t)"]
["PSC8.8.7","Spoiling excavated pavement material not required for backfilling","cubic metre (m3)"]
["PSC8.8.8","Application of waterproofing sealant to asphalt patches","litre (ℓ)"]
["CHAPTER 9: ASPHALT LAYERS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["ITEM","DESCRIPTION","UNIT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["SECTION 9.1: ASPHALT LAYERS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C9.1.1","Asphalt mix designs"]
["C9.1.1.2","Sand skeletal mixes:"]
["C9.1.1.2(e)","Level II mix design (Specialist mix specified by the Engineer)","lump sum"]
["C9.1.3","Application of bond coat"]
["C9.1.3.1","Stable–grade 30% net bitumen emulsion (cationic or anionic). Applied with a calibrated distributer ","litre (ℓ)"]
["C9.1.3.4","Polymer modified bitumen emulsion bond coat (0.45l/m²) ","litre (ℓ)"]
["C9.1.3.5","Polymer modified bitumen emulsion tack coat (0.6l/m² to old dry bituminous surfaces) ","litre (ℓ)"]
["C9.1.8","Surfacing of bridge decks"]
["C9.1.8.2","Surfacing  "]
["C9.1.8.2(a)","Surfacing at bridge joint with PG58V-22 (A-E2), 10mm NMPS, level II, sand skeletal mix"]
["C9.1.8.2(a)(i)","25mm minimum thickness","ton (t)"]
["C9.1.8.2(a)(ii)","30mm minimum thickness","ton (t)"]
["C9.1.8.2(a)(iii)","40mm minimum thickness","ton (t)"]
["C9.1.8.2(a)(iv)","50mm minimum thickness","ton (t)"]
["C9.1.8.2(a)(v)","60mm minimum thickness","ton (t)"]
["C9.1.10","Variation rates  "]
["C9.1.10.1","Bitumen "]
["C9.1.10.1(a)","35/50","ton (t)"]
["C9.1.10.1(b)","50/70","ton (t)"]
["C9.1.10.1(c)","70/100","ton (t)"]
["C9.1.10.2","Aggregate   ","ton (t)"]
["C9.1.10.3","Active filler"]
["C9.1.10.3(a)","Cement","ton (t)"]
["C9.1.10.3(b)","Lime","ton (t)"]
["C9.1.12","Asphalt reinforcing - complete (a high strength, open fibreglass grid, suitable for use as an asphalt reinforcing interlayer)","square metre (m2)"]
["CHAPTER 11: ANCILLARY ROAD WORKS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["ITEM","DESCRIPTION","UNIT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["SECTION 11.1: PITCHING, STONEWORK, CAST IN SITU CONCRETE FOR PROTECTION AGAINST EROSION",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.1.2","Stone pitching",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.1.2.1","Plain stone pitching",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.1.2.1(a)","Method 1","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.1.2.1(b)","Method 2","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.1.2.2","Grouted stone pitching with mortar","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.1.2.3","Grouted stone pitching on a concrete bed ","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC11.1.4","Stone masonry walls:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC11.1.4.4","Repair of stone retaining walls with heritage status","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["CHAPTER 11: ANCILLARY ROAD WORKS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["ITEM","DESCRIPTION","UNIT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["SECTION 11.2: NON-STRUCTURAL GABIONS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.2.2","Surface preparation for bedding the gabion boxes and mattresses","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC11.2.3","Gabion boxes and mattresses:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.2.3.1","Galvanized gabion boxes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.2.3.1(a)","1m x 1m x 1m","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.2.3.1(b)","2m x 1m x 1m","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.2.3.1(c)","1.5m x 1m x 1m","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.2.3.1(d)","1m x 1m x 0.5m","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.2.3.2","PVC coated gabion boxes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.2.3.2(a)","1m x 1m x 1m","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.2.3.2(b)","2m x 1m x 1m","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.2.3.2(c)","1.5m x 1m x 1m","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.2.3.2(d)","1m x 1m x 0.5m","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.2.3.3","Galvanized gabion mattresses ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.2.3.3(a)","2m x 1m x 0.3m","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.2.3.3(b)","3m x 1m x 0.3m","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.2.3.3(c)","6m x 2m x 0.17m","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.2.3.4","PVC-coated gabion mattresses",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.2.3.4(a)","2m x 1m x 0.3m","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.2.3.4(b)","3m x 1m x 0.3m","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.2.3.4(c)","6m x 2m x 0.17m","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC11.2.3.5","Repair of existing gabion boxes and mattresses using existing gabion rock","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.2.4","Geotextile (synthetic fibre grade 3 filter fabric)","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["CHAPTER 11: ANCILLARY ROAD WORKS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["ITEM","DESCRIPTION","UNIT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["SECTION 11.4: ROAD RESTRAINT SYSTEMS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.4.1","Erecting of guardrails at 3,81m spacing",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.4.1.1","Complete galvanized system compliant to SANS 1350:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.4.1.1(a)","On timber posts","metre (m)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.4.1.2","Terminal sections for 3,81 guardrails comprising of:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.4.1.2(a)","End wings to SANS 1350","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.4.1.2(b)","Bullnoses to SANS 1350","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.4.1.2(c)","Bridge adapters to SANS 1350 ","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.4.1.2(f)","Bridge adaptors (including extra rails and posts) (S5023-5003)","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.4.5","Additional guardrail posts for 3,81m systems:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.4.5.1","Timber","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.4.6","Reflective plates",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.4.6.1","Steel plates","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.4.7","Removing existing guardrails:","metre (m)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.4.8","Renovating guardrail material: ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.4.8.1","Painting guardrails, end wings and bullnoses","metre (m)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.4.14","Nailing of gang nail plates on top of timber guardrail posts","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["CHAPTER 11: ANCILLARY ROAD WORKS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["ITEM","DESCRIPTION","UNIT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["SECTION 11.5: FENCING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC11.5.9","Repairing existing fences ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC11.5.9.1","Repairing existing fences ","provisional sum",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC11.5.9.2","Handling cost, profit and all other charges in respect of item PSC11.5.9.2","percentage (%)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["CHAPTER 11: ANCILLARY ROAD WORKS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["ITEM","DESCRIPTION","UNIT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["SECTION 11.6: ROAD SIGNS ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC11.6.1","Road signboards with painted or coloured semi-matt background. Symbols, lettering and borders in semi- matt black or in Class I retro-reflective material, where the sign board is constructed from:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC11.6.1.7","Regulatory signs, permanent ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC11.6.1.7(a)","600mm diameter ","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC11.6.1.7(b)","900mm diameter","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC11.6.1.7(c)","1200mm diameter","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC11.6.1.9","Warning signs, permanent ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC11.6.1.9(a)","600mm size ","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC11.6.1.9(b)","900mm size ","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC11.6.1.9(c)","1200mm size","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC11.6.1.9(d)","1500mm size","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC11.6.1.11","Supplementary plates to permanent regulatory or warning signs ","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["CHAPTER 13: STRUCTURES",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["ITEM","DESCRIPTION","UNIT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["SECTION 13.1: FOUNDATIONS ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.1.3","Excavation:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.1.3.1","Excavating soft material situated within the following successive depth ranges:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.1.3.1(a)","0m up to 1,5m","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.1.3.1(b)","> 1,5m and < 3,0m","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.1.3.1(c)","> 3,0m and < 4,5m","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.1.3.2","Extra over subitem C13.1.3.1 for excavation in hard material  irrespective of depth","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.1.3.4","Extra over subitem C13.1.3.1 for excavation by hand","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.1.3.5","Extra over subitem C13.1.3.1 for excavation in restricted areas","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.1.6","Access and drainage:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.1.6.1","Access","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.1.6.2","Drainage","day",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C13.1.7","Backfill to excavations utilising:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C13.1.7.1","Material from excavation","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C13.1.7.2","Imported material","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C13.1.7.3","Soil cement","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C13.1.10","Haul in excess of 1,0 km on excavated material and on material imported for backfill, foundation fill and fill for caissons","cubic metre kilometre (m3.km)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C13.1.14","Foundation fill consisting of:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C13.1.14.1","Rock fill","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C13.1.14.2","Crushed-stone fill","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C13.1.14.3","Compacted granular material","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C13.1.14.4","Mass concrete (Class C12/15-20)","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C13.1.14.5","Concrete blinding (max 75mm thick, C12/15-20)","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["CHAPTER 13: STRUCTURES",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["ITEM","DESCRIPTION","UNIT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["SECTION 13.2: FALSEWORK, FORMWORK AND CONCRETE FINISH",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2","Vertical formwork to provide (class of finish indicated as F1, F2, F3 or board) surface finish to (description of member to which applicable)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.1","Class F1 finish to elements as indicated",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.1(a)","Abutments","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.1(b)","Piers","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.1(c)","Walls","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.1(d)","Parapets including endblocks","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.1(e)","Deck longitudinal members","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.1(f)","Deck transverse members","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.1(g)","Deck slabs","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.1(h)","Foundations","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.1(i)","Sidewalks","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.1(j)","Culvert barrel","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.1(k)","Culvert headwall","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.1(l)","Apron slabs and cut off walls","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.2","Class F2 finish to elements as indicated",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.2(a)","Abutments","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.2(b)","Piers","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.2(c)","Walls","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.2(d)","Parapets including endblocks","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.2(e)","Deck longitudinal members","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.2(f)","Deck transverse members","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.2(g)","Deck slabs","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.2(h)","Foundations","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.2(i)","Sidewalks","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.2(j)","Culvert barrel","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.2(k)","Culvert headwall","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.2(l)","Apron slabs and cut off walls","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.3","Class F3 finish to elements as indicated",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.3(a)","Abutments","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.3(b)","Piers","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.3(c)","Walls","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.3(d)","Parapets including endblocks","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.3(e)","Deck longitudinal members","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.3(f)","Deck transverse members","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.3(g)","Deck slabs","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.3(h)","Foundations","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.3(i)","Sidewalks","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.3(j)","Culvert barrel","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.3(k)","Culvert headwall","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.3(l)","Apron slabs and cut off walls","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.3","Horizontal formwork to provide (class of finish Indicated as F1, F2, F3 or board) surface finish to (description of member to which applicable)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.3.1","Class F1 finish to elements as indicated",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.3.1(a)","Abutments","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.3.1(b)","Piers","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.3.1(c)","Walls","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.3.1(d)","Parapets including endblocks","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.3.1(e)","Deck longitudinal members","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.3.1(f)","Deck transverse members","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.3.1(g)","Deck slabs","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.3.1(h)","Foundations","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.3.1(i)","Sidewalks","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.3.1(j)","Culvert barrel","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.3.1(k)","Culvert headwall","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.3.1(l)","Apron slabs and cut off walls","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.3.2","Class F2 finish to elements as indicated",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.3.2(a)","Abutments","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.3.2(b)","Piers","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.3.2(c)","Walls","square metre (m2)"]
["PSC13.2.3.2(d)","Parapets including endblocks","square metre (m2)"]
["PSC13.2.3.2(e)","Deck longitudinal members","square metre (m2)"]
["PSC13.2.3.2(f)","Deck transverse members","square metre (m2)"]
["PSC13.2.3.2(g)","Deck slabs","square metre (m2)"]
["PSC13.2.3.2(h)","Foundations","square metre (m2)"]
["PSC13.2.3.2(i)","Sidewalks","square metre (m2)"]
["PSC13.2.3.2(j)","Culvert barrel","square metre (m2)"]
["PSC13.2.3.2(k)","Culvert headwall","square metre (m2)"]
["PSC13.2.3.2(l)","Apron slabs and cut off walls","square metre (m2)"]
["PSC13.2.3.3","Class F3 finish to elements as indicated"]
["PSC13.2.3.3(a)","Abutments","square metre (m2)"]
["PSC13.2.3.3(b)","Piers","square metre (m2)"]
["PSC13.2.3.3(c)","Walls","square metre (m2)"]
["PSC13.2.3.3(d)","Parapets including endblocks","square metre (m2)"]
["PSC13.2.3.3(e)","Deck longitudinal members","square metre (m2)"]
["PSC13.2.3.3(f)","Deck transverse members","square metre (m2)"]
["PSC13.2.3.3(g)","Deck slabs","square metre (m2)"]
["PSC13.2.3.3(h)","Foundations","square metre (m2)"]
["PSC13.2.3.3(i)","Sidewalks","square metre (m2)"]
["PSC13.2.3.3(j)","Culvert barrel","square metre (m2)"]
["PSC13.2.3.3(k)","Culvert headwall","square metre (m2)"]
["PSC13.2.3.3(l)","Apron slabs and cut off walls","square metre (m2)"]
["PSC13.2.4","Inclined formwork to provide (class of finish indicated as F1, F2, F3 or board) surface finish to (description of member to which applicable)"]
["PSC13.2.4.1","Class F1 finish to elements as indicated"]
["PSC13.2.4.1(a)","Abutments","square metre (m2)"]
["PSC13.2.4.1(b)","Piers","square metre (m2)"]
["PSC13.2.4.1(c)","Walls","square metre (m2)"]
["PSC13.2.4.1(d)","Parapets including endblocks","square metre (m2)"]
["PSC13.2.4.1(e)","Deck longitudinal members","square metre (m2)"]
["PSC13.2.4.1(f)","Deck transverse members","square metre (m2)"]
["PSC13.2.4.1(g)","Deck slabs","square metre (m2)"]
["PSC13.2.4.1(h)","Foundations","square metre (m2)"]
["PSC13.2.4.1(i)","Sidewalks","square metre (m2)"]
["PSC13.2.4.1(j)","Culvert barrel","square metre (m2)"]
["PSC13.2.4.1(k)","Culvert headwall","square metre (m2)"]
["PSC13.2.4.1(l)","Apron slabs and cut off walls","square metre (m2)"]
["PSC13.2.4.2","Class F2 finish to elements as indicated"]
["PSC13.2.4.2(a)","Abutments","square metre (m2)"]
["PSC13.2.4.2(b)","Piers","square metre (m2)"]
["PSC13.2.4.2(c)","Walls","square metre (m2)"]
["PSC13.2.4.2(d)","Parapets including endblocks","square metre (m2)"]
["PSC13.2.4.2(e)","Deck longitudinal members","square metre (m2)"]
["PSC13.2.4.2(f)","Deck transverse members","square metre (m2)"]
["PSC13.2.4.2(g)","Deck slabs","square metre (m2)"]
["PSC13.2.4.2(h)","Foundations","square metre (m2)"]
["PSC13.2.4.2(i)","Sidewalks","square metre (m2)"]
["PSC13.2.4.2(j)","Culvert barrel","square metre (m2)"]
["PSC13.2.4.2(k)","Culvert headwall","square metre (m2)"]
["PSC13.2.4.2(l)","Apron slabs and cut off walls","square metre (m2)"]
["PSC13.2.4.3","Class F3 finish to elements as indicated"]
["PSC13.2.4.3(a)","Abutments","square metre (m2)"]
["PSC13.2.4.3(b)","Piers","square metre (m2)"]
["PSC13.2.4.3(c)","Walls","square metre (m2)"]
["PSC13.2.4.3(d)","Parapets including endblocks","square metre (m2)"]
["PSC13.2.4.3(e)","Deck longitudinal members","square metre (m2)"]
["PSC13.2.4.3(f)","Deck transverse members","square metre (m2)"]
["PSC13.2.4.3(g)","Deck slabs","square metre (m2)"]
["PSC13.2.4.3(h)","Foundations","square metre (m2)"]
["PSC13.2.4.3(i)","Sidewalks","square metre (m2)"]
["PSC13.2.4.3(j)","Culvert barrel","square metre (m2)"]
["PSC13.2.4.3(k)","Culvert headwall","square metre (m2)"]
["PSC13.2.4.3(l)","Apron slabs and cut off walls","square metre (m2)"]
["C13.2.6","Formwork to form open joints (description of member to which applicable, and location) "]
["C13.2.6.1","Parapets at expansion joints","square metre (m2)"]
["CHAPTER 13: STRUCTURES"]
["ITEM","DESCRIPTION","UNIT"]
["SECTION 13.3: STEEL REINFORCEMENT"]
["C13.3.1","Reinforcement for:"]
["C13.3.1.1","Parapets including endblocks and Precast Balustrade Types A to Q (to drawing S5023-5010)"]
["C13.3.1.1(a)","Mild-steel bars","ton (t)"]
["C13.3.1.1(b)","High-yield-stress-steel bars (deformed Y-bars)","ton (t)"]
["C13.3.1.2","Precast balustrade top rails Types A to Q (to drawing S5023-5007)"]
["C13.3.1.2(a)","Mild-steel bars","ton (t)"]
["C13.3.1.2(b)","High-yield-stress-steel bars (deformed Y-bars)","ton (t)"]
["C13.3.1.3","Abutments"]
["C13.3.1.3(a)","Mild-steel bars","ton (t)"]
["C13.3.1.3(b)","High-yield-stress-steel bars (deformed Y-bars)","ton (t)"]
["C13.3.1.3(c)","Welded Steel Fabric","kilogram (kg)"]
["C13.3.1.4","Piers"]
["C13.3.1.4(a)","Mild-steel bars","ton (t)"]
["C13.3.1.4(b)","High-yield-stress-steel bars (deformed Y-bars)","ton (t)"]
["C13.3.1.4(c)","Welded Steel Fabric","kilogram (kg)"]
["C13.3.1.5","Walls"]
["C13.3.1.5(a)","Mild-steel bars","ton (t)"]
["C13.3.1.5(b)","High-yield-stress-steel bars (deformed Y-bars)","ton (t)"]
["C13.3.1.5(c)","Welded Steel Fabric","kilogram (kg)"]
["C13.3.1.6","Deck"]
["C13.3.1.6(a)","Mild-steel bars","ton (t)"]
["C13.3.1.6(b)","High-yield-stress-steel bars (deformed Y-bars)","ton (t)"]
["C13.3.1.6(c)","Welded Steel Fabric","kilogram (kg)"]
["C13.3.1.7","Foundations"]
["C13.3.1.7(a)","Mild-steel bars","ton (t)"]
["C13.3.1.7(b)","High-yield-stress-steel bars (deformed Y-bars)","ton (t)"]
["C13.3.1.7(c)","Welded Steel Fabric","kilogram (kg)"]
["C13.3.1.8","Culvert barrels"]
["C13.3.1.8(a)","Mild-steel bars","ton (t)"]
["C13.3.1.8(b)","High-yield-stress-steel bars (deformed Y-bars)","ton (t)"]
["C13.3.1.8(c)","Welded Steel Fabric","kilogram (kg)"]
["C13.3.1.9","Culvert headwalls"]
["C13.3.1.9(a)","Mild-steel bars","ton (t)"]
["C13.3.1.9(b)","High-yield-stress-steel bars (deformed Y-bars)","ton (t)"]
["C13.3.1.9(c)","Welded Steel Fabric","kilogram (kg)"]
["C13.3.1.10","Apron slabs and cut off walls"]
["C13.3.1.10(a)","Mild-steel bars","ton (t)"]
["C13.3.1.10(b)","High-yield-stress-steel bars (deformed Y-bars)","ton (t)"]
["C13.3.1.10(c)","Welded Steel Fabric","kilogram (kg)"]
["C13.3.4","Extra-over item C13.3.1 (a), (b), etc. for galvanising of reinforcement    ","ton (t)"]
["CHAPTER 13: STRUCTURES"]
["ITEM","DESCRIPTION","UNIT"]
["SECTION 13.4: CONCRETE"]
["C13.4.1","Cast in situ concrete (Class of concrete and use or position in structure stated): "]
["C13.4.1.1","Strength concrete (class C):"]
["C13.4.1.1(a)","C12/15-20"]
["C13.4.1.1(a)(i)","Abutments","cubic metre (m3)"]
["C13.4.1.1(a)(ii)","Piers","cubic metre (m3)"]
["C13.4.1.1(a)(iii)","Walls","cubic metre (m3)"]
["C13.4.1.1(a)(iv)","Parapets","cubic metre (m3)"]
["C13.4.1.1(a)(v)","Deck longitudinal members","cubic metre (m3)"]
["C13.4.1.1(a)(vi)","Deck transverse members","cubic metre (m3)"]
["C13.4.1.1(a)(vii)","Deck slabs","cubic metre (m3)"]
["C13.4.1.1(a)(iiv)","Foundations","cubic metre (m3)"]
["C13.4.1.1(a)(iv)","Sidewalks","cubic metre (m3)"]
["C13.4.1.1(a)(v)","Culvert barrel","cubic metre (m3)"]
["C13.4.1.1(a)(vi)","Culvert headwall","cubic metre (m3)"]
["C13.4.1.1(a)(vii)","Apron slabs and cut off walls","cubic metre (m3)"]
["C13.4.1.1(b)","C25/30-20"]
["C13.4.1.1(b)(i)","Abutments","cubic metre (m3)"]
["C13.4.1.1(b)(ii)","Piers","cubic metre (m3)"]
["C13.4.1.1(b)(iii)","Walls","cubic metre (m3)"]
["C13.4.1.1(b)(iv)","Parapets","cubic metre (m3)"]
["C13.4.1.1(b)(v)","Deck longitudinal members","cubic metre (m3)"]
["C13.4.1.1(b)(vi)","Deck transverse members","cubic metre (m3)"]
["C13.4.1.1(b)(vii)","Deck slabs","cubic metre (m3)"]
["C13.4.1.1(b)(iiv)","Foundations","cubic metre (m3)"]
["C13.4.1.1(b)(iv)","Sidewalks","cubic metre (m3)"]
["C13.4.1.1(b)(v)","Culvert barrel","cubic metre (m3)"]
["C13.4.1.1(b)(vi)","Culvert headwall","cubic metre (m3)"]
["C13.4.1.1(b)(vii)","Apron slabs and cut off walls","cubic metre (m3)"]
["C13.4.1.1(c)","C35/40-20"]
["C13.4.1.1(c)(i)","Abutments","cubic metre (m3)"]
["C13.4.1.1(c)(ii)","Piers","cubic metre (m3)"]
["C13.4.1.1(c)(iii)","Walls","cubic metre (m3)"]
["C13.4.1.1(c)(iv)","Parapets","cubic metre (m3)"]
["C13.4.1.1(c)(v)","Deck longitudinal members","cubic metre (m3)"]
["C13.4.1.1(c)(vi)","Deck transverse members","cubic metre (m3)"]
["C13.4.1.1(c)(vii)","Deck slabs","cubic metre (m3)"]
["C13.4.1.1(c)(iiv)","Foundations","cubic metre (m3)"]
["C13.4.1.1(c)(iv)","Sidewalks","cubic metre (m3)"]
["C13.4.1.1(c)(v)","Culvert barrel","cubic metre (m3)"]
["C13.4.1.1(c)(vi)","Culvert headwall","cubic metre (m3)"]
["C13.4.1.1(c)(vii)","Apron slabs and cut off walls","cubic metre (m3)"]
["C13.4.1.2(c)","Durable concrete (class D):"]
["C13.4.1.2(a)","D25/30-XC4(100)-20"]
["C13.4.1.2(a)(i)","Abutments","cubic metre (m3)"]
["C13.4.1.2(a)(ii)","Piers","cubic metre (m3)"]
["C13.4.1.2(a)(iii)","Walls","cubic metre (m3)"]
["C13.4.1.2(a)(iv)","Parapets","cubic metre (m3)"]
["C13.4.1.2(a)(v)","Deck longitudinal members","cubic metre (m3)"]
["C13.4.1.2(a)(vi)","Deck transverse members","cubic metre (m3)"]
["C13.4.1.2(a)(vii)","Deck slabs","cubic metre (m3)"]
["C13.4.1.2(a)(iiv)","Foundations","cubic metre (m3)"]
["C13.4.1.2(a)(iv)","Sidewalks","cubic metre (m3)"]
["C13.4.1.2(a)(v)","Culvert barrel","cubic metre (m3)"]
["C13.4.1.2(a)(vi)","Culvert headwall","cubic metre (m3)"]
["C13.4.1.2(a)(vii)","Apron slabs and cut off walls","cubic metre (m3)"]
["C13.4.1.2(b)","D35/40-XC4(100)-20"]
["C13.4.1.2(b)(i)","Abutments","cubic metre (m3)"]
["C13.4.1.2(b)(ii)","Piers","cubic metre (m3)"]
["C13.4.1.2(b)(iii)","Walls","cubic metre (m3)"]
["C13.4.1.2(b)(iv)","Parapets","cubic metre (m3)"]
["C13.4.1.2(b)(v)","Deck longitudinal members","cubic metre (m3)"]
["C13.4.1.2(b)(vi)","Deck transverse members","cubic metre (m3)"]
["C13.4.1.2(b)(vii)","Deck slabs","cubic metre (m3)"]
["C13.4.1.2(b)(iiv)","Foundations","cubic metre (m3)"]
["C13.4.1.2(b)(iv)","Sidewalks","cubic metre (m3)"]
["C13.4.1.2(b)(v)","Culvert barrel","cubic metre (m3)"]
["C13.4.1.2(b)(vi)","Culvert headwall","cubic metre (m3)"]
["C13.4.1.2(b)(vii)","Apron slabs and cut off walls","cubic metre (m3)"]
["C13.4.1.2(c)","D25/30-XS1(100)-20"]
["C13.4.1.2(c)(i)","Abutments","cubic metre (m3)"]
["C13.4.1.2(c)(ii)","Piers","cubic metre (m3)"]
["C13.4.1.2(c)(iii)","Walls","cubic metre (m3)"]
["C13.4.1.2(c)(iv)","Parapets","cubic metre (m3)"]
["C13.4.1.2(c)(v)","Deck longitudinal members","cubic metre (m3)"]
["C13.4.1.2(c)(vi)","Deck transverse members","cubic metre (m3)"]
["C13.4.1.2(c)(vii)","Deck slabs","cubic metre (m3)"]
["C13.4.1.2(c)(iiv)","Foundations","cubic metre (m3)"]
["C13.4.1.2(c)(iv)","Sidewalks","cubic metre (m3)"]
["C13.4.1.2(c)(v)","Culvert barrel","cubic metre (m3)"]
["C13.4.1.2(c)(vi)","Culvert headwall","cubic metre (m3)"]
["C13.4.1.2(c)(vii)","Apron slabs and cut off walls","cubic metre (m3)"]
["C13.4.1.2(d)","D35/40-XS1(100)-20"]
["C13.4.1.2(d)(i)","Abutments","cubic metre (m3)"]
["C13.4.1.2(d)(ii)","Piers","cubic metre (m3)"]
["C13.4.1.2(d)(iii)","Walls","cubic metre (m3)"]
["C13.4.1.2(d)(iv)","Parapets","cubic metre (m3)"]
["C13.4.1.2(d)(v)","Deck longitudinal members","cubic metre (m3)"]
["C13.4.1.2(d)(vi)","Deck transverse members","cubic metre (m3)"]
["C13.4.1.2(d)(vii)","Deck slabs","cubic metre (m3)"]
["C13.4.1.2(d)(iiv)","Foundations","cubic metre (m3)"]
["C13.4.1.2(d)(iv)","Sidewalks","cubic metre (m3)"]
["C13.4.1.2(d)(v)","Culvert barrel","cubic metre (m3)"]
["C13.4.1.2(d)(vi)","Culvert headwall","cubic metre (m3)"]
["C13.4.1.2(d)(vii)","Apron slabs and cut off walls","cubic metre (m3)"]
["PSC13.4.5","Curing and surface protection of cast in situ concrete, as and where specifically required:"]
["PSC13.4.5.1","Curing using formwork that is retained in place for full curing period"]
["PSC13.4.5.1(a)","Abutments","square metre (m2)"]
["PSC13.4.5.1(b)","Piers","square metre (m2)"]
["PSC13.4.5.1(c)","Walls","square metre (m2)"]
["PSC13.4.5.1(d)","Parapets","square metre (m2)"]
["PSC13.4.5.1(e)","Deck longitudinal members","square metre (m2)"]
["PSC13.4.5.1(f)","Deck transverse members","square metre (m2)"]
["PSC13.4.5.1(g)","Deck slabs","square metre (m2)"]
["PSC13.4.5.1(h)","Foundations","square metre (m2)"]
["PSC13.4.5.1(i)","Sidewalks","square metre (m2)"]
["PSC13.4.5.1(j)","Culvert barrel","square metre (m2)"]
["PSC13.4.5.1(k)","Culvert headwall","square metre (m2)"]
["PSC13.4.5.1(l)","Apron slabs and cut off walls","square metre (m2)"]
["PSC13.4.5.2","Curing using water ponding or constantly spraying exposed surfaces with water"]
["PSC13.4.5.2(a)","Abutments","square metre (m2)"]
["PSC13.4.5.2(b)","Piers","square metre (m2)"]
["PSC13.4.5.2(c)","Walls","square metre (m2)"]
["PSC13.4.5.2(d)","Parapets","square metre (m2)"]
["PSC13.4.5.2(e)","Deck longitudinal members","square metre (m2)"]
["PSC13.4.5.2(f)","Deck transverse members","square metre (m2)"]
["PSC13.4.5.2(g)","Deck slabs","square metre (m2)"]
["PSC13.4.5.2(h)","Foundations","square metre (m2)"]
["PSC13.4.5.2(i)","Sidewalks","square metre (m2)"]
["PSC13.4.5.2(j)","Culvert barrel","square metre (m2)"]
["PSC13.4.5.2(k)","Culvert headwall","square metre (m2)"]
["PSC13.4.5.2(l)","Apron slabs and cut off walls","square metre (m2)"]
["PSC13.4.5.3","Curing using an approved curing compound"]
["PSC13.4.5.3(a)","Abutments","square metre (m2)"]
["PSC13.4.5.3(b)","Piers","square metre (m2)"]
["PSC13.4.5.3(c)","Walls","square metre (m2)"]
["PSC13.4.5.3(d)","Parapets","square metre (m2)"]
["PSC13.4.5.3(e)","Deck longitudinal members","square metre (m2)"]
["PSC13.4.5.3(f)","Deck transverse members","square metre (m2)"]
["PSC13.4.5.3(g)","Deck slabs","square metre (m2)"]
["PSC13.4.5.3(h)","Foundations","square metre (m2)"]
["PSC13.4.5.3(i)","Sidewalks","square metre (m2)"]
["PSC13.4.5.3(j)","Culvert barrel","square metre (m2)"]
["PSC13.4.5.3(k)","Culvert headwall","square metre (m2)"]
["PSC13.4.5.3(l)","Apron slabs and cut off walls","square metre (m2)"]
["PSC13.4.5.4","Curing using plastic sheeting covering, covering with clean sand or absorbant moisture retaining mats"]
["PSC13.4.5.4(a)","Abutments","square metre (m2)"]
["PSC13.4.5.4(b)","Piers","square metre (m2)"]
["PSC13.4.5.4(c)","Walls","square metre (m2)"]
["PSC13.4.5.4(d)","Parapets","square metre (m2)"]
["PSC13.4.5.4(e)","Deck longitudinal members","square metre (m2)"]
["PSC13.4.5.4(f)","Deck transverse members","square metre (m2)"]
["PSC13.4.5.4(g)","Deck slabs","square metre (m2)"]
["PSC13.4.5.4(h)","Foundations","square metre (m2)"]
["PSC13.4.5.4(i)","Sidewalks","square metre (m2)"]
["PSC13.4.5.4(j)","Culvert barrel","square metre (m2)"]
["PSC13.4.5.4(k)","Culvert headwall","square metre (m2)"]
["PSC13.4.5.4(l)","Apron slabs and cut off walls","square metre (m2)"]
["PSC13.4.9","Manufacturing precast concrete members (description of member with reference to drawing)"]
["PSC13.4.9.1","Precast balustrade (drawing S5023-5010),excluding reinforcement"]
["PSC13.4.9.1(a)","Type A precast balustrade (drawing S5023-5010), excluding reinforcement","number (No.)"]
["PSC13.4.9.1(b)","Type B precast balustrade (drawing S5023-5010), excluding reinforcement","number (No.)"]
["PSC13.4.9.1(c)","Type C precast balustrade (drawing S5023-5010), excluding reinforcement","number (No.)"]
["PSC13.4.9.1(d)","Type D precast balustrade (drawing S5023-5010), excluding reinforcement","number (No.)"]
["PSC13.4.9.1(e)","Type E precast balustrade (drawing S5023-5010), excluding reinforcement","number (No.)"]
["PSC13.4.9.1(f)","Type F precast balustrade (drawing S5023-5010), excluding reinforcement","number (No.)"]
["PSC13.4.9.1(g)","Type G precast balustrade (drawing S5023-5010), excluding reinforcement","number (No.)"]
["PSC13.4.9.1(h)","Type H precast balustrade (drawing S5023-5010), excluding reinforcement","number (No.)"]
["PSC13.4.9.1(i)","Type J precast balustrade (drawing S5023-5010), excluding reinforcement","number (No.)"]
["PSC13.4.9.1(j)","Type K precast balustrade (drawing S5023-5010), excluding reinforcement","number (No.)"]
["PSC13.4.9.1(k)","Type L precast balustrade (drawing S5023-5010), excluding reinforcement","number (No.)"]
["PSC13.4.9.1(l)","Type M precast balustrade (drawing S5023-5010), excluding reinforcement","number (No.)"]
["PSC13.4.9.1(m)","Type N precast balustrade (drawing S5023-5010), excluding reinforcement","number (No.)"]
["PSC13.4.9.1(n)","Type P precast balustrade (drawing S5023-5010), excluding reinforcement","number (No.)"]
["PSC13.4.9.1(o)","Type Q precast balustrade (drawing S5023-5010), excluding reinforcement","number (No.)"]
["PSC13.4.9.2","Precast top rails (drawing S5023-5007),excluding reinforcement"]
["PSC13.4.9.2(a)","Type A precast top rails (drawing S5023-5007), excluding reinforcement","number (No.)"]
["PSC13.4.9.2(b)","Type B precast top rails (drawing S5023-5007), excluding reinforcement","number (No.)"]
["PSC13.4.9.2(c)","Type C precast top rails (drawing S5023-5007), excluding reinforcement","number (No.)"]
["PSC13.4.9.2(d)","Type D precast top rails (drawing S5023-5007), excluding reinforcement","number (No.)"]
["PSC13.4.9.2(e)","Type E precast top rails (drawing S5023-5007), excluding reinforcement","number (No.)"]
["PSC13.4.9.2(f)","Type F precast top rails (drawing S5023-5007), excluding reinforcement","number (No.)"]
["PSC13.4.9.2(g)","Type G precast top rails (drawing S5023-5007), excluding reinforcement","number (No.)"]
["PSC13.4.9.2(h)","Type H precast top rails (drawing S5023-5007), excluding reinforcement","number (No.)"]
["PSC13.4.9.2(i)","Type J precast top rails (drawing S5023-5007), excluding reinforcement","number (No.)"]
["PSC13.4.9.2(j)","Type K precast top rails (drawing S5023-5007), excluding reinforcement","number (No.)"]
["PSC13.4.9.2(k)","Type L precast top rails (drawing S5023-5007), excluding reinforcement","number (No.)"]
["PSC13.4.9.2(l)","Type M precast top rails (drawing S5023-5007), excluding reinforcement","number (No.)"]
["PSC13.4.9.2(m)","Type N precast top rails (drawing S5023-5007), excluding reinforcement","number (No.)"]
["PSC13.4.9.2(n)","Type P precast top rails (drawing S5023-5007), excluding reinforcement","number (No.)"]
["PSC13.4.9.2(o)","Type Q precast top rails (drawing S5023-5007), excluding reinforcement","number (No.)"]
["PSC13.4.11","Transporting and erecting precast concrete members including complete installation (description of member with reference to drawing)"]
["PSC13.4.11.1","Precast balustrades (drawing S5023-5010) "]
["PSC13.4.11.1(a)","Type A precast balustrade (drawing S5023-5010) approx 970 kg","number (No.)"]
["PSC13.4.11.1(b)","Type B precast balustrade (drawing S5023-5010) approx 1200 kg","number (No.)"]
["PSC13.4.11.1(c)","Type C precast balustrade (drawing S5023-5010) approx 1360 kg","number (No.)"]
["PSC13.4.11.1(d)","Type D precast balustrade (drawing S5023-5010) approx 1500 kg","number (No.)"]
["PSC13.4.11.1(e)","Type E precast balustrade (drawing S5023-5010) approx 1800 kg","number (No.)"]
["PSC13.4.11.1(f)","Type F precast balustrade (drawing S5023-5010) approx 2000 kg","number (No.)"]
["PSC13.4.11.1(g)","Type G precast balustrade (drawing S5023-5010) approx 2080 kg","number (No.)"]
["PSC13.4.11.1(h)","Type H precast balustrade (drawing S5023-5010) approx 2200 kg","number (No.)"]
["PSC13.4.11.1(i)","Type J precast balustrade (drawing S5023-5010) approx 2340 kg","number (No.)"]
["PSC13.4.11.1(j)","Type K precast balustrade (drawing S5023-5010) approx 2460 kg","number (No.)"]
["PSC13.4.11.1(k)","Type L precast balustrade (drawing S5023-5010) approx 2600 kg","number (No.)"]
["PSC13.4.11.1(l)","Type M precast balustrade (drawing S5023-5010) approx 2800 kg","number (No.)"]
["PSC13.4.11.1(m)","Type N precast balustrade (drawing S5023-5010) approx 2700 kg","number (No.)"]
["PSC13.4.11.1(n)","Type P precast balustrade (drawing S5023-5010) approx 2800 kg","number (No.)"]
["PSC13.4.11.1(o)","Type Q precast balustrade (drawing S5023-5010) approx 3000 kg","number (No.)"]
["PSC13.4.11.2","Precast top rails (drawing S5023-5007)"]
["PSC13.4.11.2(a)","Type A precast top rail (drawing S5023-5007) ","number (No.)"]
["PSC13.4.11.2(b)","Type B precast top rail (drawing S5023-5007)","number (No.)"]
["PSC13.4.11.2(c)","Type C precast top rail (drawing S5023-5007) ","number (No.)"]
["PSC13.4.11.2(d)","Type D precast top rail (drawing S5023-5007) ","number (No.)"]
["PSC13.4.11.2(e)","Type E precast top rail (drawing S5023-5007) ","number (No.)"]
["PSC13.4.11.2(f)","Type F precast top rail (drawing S5023-5007) ","number (No.)"]
["PSC13.4.11.2(g)","Type G precast top rail (drawing S5023-5007) ","number (No.)"]
["PSC13.4.11.2(h)","Type H precast top rail (drawing S5023-5007) ","number (No.)"]
["PSC13.4.11.2(i)","Type J precast top rail (drawing S5023-5007) ","number (No.)"]
["PSC13.4.11.2(j)","Type K precast top rail (drawing S5023-5007) ","number (No.)"]
["PSC13.4.11.2(k)","Type L precast top rail (drawing S5023-5007) ","number (No.)"]
["PSC13.4.11.2(l)","Type M precast top rail (drawing S5023-5007) ","number (No.)"]
["PSC13.4.11.2(m)","Type N precast top rail (drawing S5023-5007) ","number (No.)"]
["PSC13.4.11.2(n)","Type P precast top rail (drawing S5023-5007) ","number (No.)"]
["PSC13.4.11.2(o)","Type Q precast top rail (drawing S5023-5007) ","number (No.)"]
["CHAPTER 13: STRUCTURES"]
["ITEM","DESCRIPTION","UNIT"]
["SECTION 13.6: BEARINGS"]
["PSC13.6.1","Bearings:"]
["PSC13.6.1.1","Bearings (description of each type and class)"]
["PSC13.6.1.1(a)","Elastomeric bearings (200 x 150mm x 48mm)","number (No.)"]
["PSC13.6.1.1(b)","Elastomeric bearings (300 x 150mm x 48mm)","number (No.)"]
["PSC13.6.1.1(c) ","Elastomeric bearings (300 x 200mm x 61mm)","number (No.)"]
["PSC13.6.1.1(d)","Elastomeric bearings (300 x 250mm x 61mm)","number (No.)"]
["PSC13.6.1.1(e)","Elastomeric bearings (400 x 300mm x 61mm)","number (No.)"]
["PSC13.6.1.1(f) ","Elastomeric bearings (400 x 500mm x 77mm)","number (No.)"]
["PSC13.6.1.1(g)","Elastomeric bearings (600 x 450mm x 72mm)","number (No.)"]
["CHAPTER 13: STRUCTURES"]
["ITEM","DESCRIPTION","UNIT"]
["SECTION 13.7: JOINTS"]
["C13.7.1","Expansion joints:"]
["C13.7.1.1","Description of joint"]
["C13.7.1.1(a)","Preformed elastomeric compression seal joint"]
["C13.7.1.1(a)(i)","Up to 20mm width","metre (m)"]
["C13.7.1.1(a)(ii)","20 - 40mm width","metre (m)"]
["C13.7.1.1(a)(i)","40 - 60mm width","metre (m)"]
["C13.7.1.1(a)(ii)","60 - 80mm width","metre (m)"]
["C13.7.1.1(b)","Silicone joint seal (approved silicone sealant including backing chord in accordance with Clause A6.1.5.7c and applied in accordance with the manufacturer's instructions)"]
["C13.7.1.1(b)(i)","Up to 20mm width","metre (m)"]
["C13.7.1.1(b)(ii)","20 - 40mm width","metre (m)"]
["C13.7.1.1(b)(i)","40 - 60mm width","metre (m)"]
["C13.7.1.1(b)(ii)","60 - 80mm width","metre (m)"]
["PSC13.7.4","Sealing joints with:"]
["C13.7.4.1","Sealant (approved silicone sealant including backing chord in accordance with Clause A6.1.5.7c)"]
["C13.7.4.1(a)","0 - 10mm width","metre (m)"]
["C13.7.4.1(b)","10 - 20mm width","metre (m)"]
["PSC13.7.4.3","Filter fabric strips (150mm wide, 340g/m², preimpregnated with bituminous emulsion and bonded across butt-joints using a 60% bituminous emulsion)","metre (m)"]
["PSC13.7.5","Supply and installation of Agrément South Africa certified proprietary expansion joints"]
["PSC13.7.5.1","Claw and other modular joints in nosings"]
["PSC13.7.5.1(a)","40mm claw joint","metre (m)"]
["PSC13.7.5.1(b)","80mm claw joint","metre (m)"]
["PSC13.7.5.2","Asphaltic plug type joints (drawings DET2.1, DET2.2, DET2.3)"]
["PSC13.7.5.2(a)","300mm x 50mm","metre (m)"]
["PSC13.7.5.2(b)","400mm x 75mm","metre (m)"]
["PSC13.7.5.2(c) ","500mm x 100mm","metre (m)"]
["PSC13.7.5.2(g)","Extra over for variation in joint depth of asphaltic joints","litre (ℓ)"]
["PSC13.7.11","Reinstating of expansion gaps in concrete elements ","litre (ℓ)"]
["CHAPTER 13: STRUCTURES"]
["ITEM","DESCRIPTION","UNIT"]
["SECTION 13.8: ANCILLARY STRUCTURAL ELEMENTS"]
["C13.8.5","Steel railings (to detail S5023-5002)","metre (m)"]
["PSC13.8.7","Numbers for structures: (refer to drawings)"]
["C13.8.7.3","Numbers formed in concrete (to detail S5023-5006)","number (No.)"]
["PSC13.8.7.5","Numbers inscribed in existing concrete (to detail S5023-5006)","number (No.)"]
["C13.8.8","Cast in situ no-fines concrete (class of concrete indicated)"]
["C13.8.8.1","C12/15-20","cubic metre (m3)"]
["C13.8.8.2","C25/30-20","cubic metre (m3)"]
["C13.8.8.2","C35/40-20","cubic metre (m3)"]
["C13.8.10","Drainage pipes and weep holes:"]
["C13.8.10.1","Drainage pipes:"]
["C13.8.10.1(a)","uPVC 75-150mm in diameter","metre (m)"]
["C13.8.10.1(b)","uPVC 150-250mm in diameter","metre (m)"]
["C13.8.10.2","Weep holes:"]
["C13.8.10.2(a)","uPVC up to 100mm in diameter","metre (m)"]
["C13.8.12","Synthetic-fibre filter fabric (geotextile grade 1) ","square metre (m²)"]
["C13.8.15","Drainage strips (150mm filter elements)","metre (m)"]
["C13.8.16","Perforated drainage pipes: "]
["C13.8.16.1","65mm diameter perforated drainage pipe wrapped in grade 1 geotextile filter fabric","metre (m)"]
["CHAPTER 13: STRUCTURES"]
["ITEM","DESCRIPTION","UNIT"]
["SECTION 13.12: STRUCTURAL STEEL PROTECTIVE TREATMENT OF MAJOR STRUCTURES"]
["PSC13.12.1","Steelwork protective system:"]
["PSC13.12.1.1","System 6 (COTO section PSA13.12.7.15) or similar approved to existing steelwork on bridges","square metre (m2)"]
["PSC13.12.1.2","System 6 (COTO section PSA13.12.7.15) or similar approved to existing steel handrails ","square metre (m2)"]
["CHAPTER 14: REPAIR OF STRUCTURES"]
["ITEM","DESCRIPTION","UNIT"]
["SECTION 14.1: ACCESS FOR BRIDGE REHABILITATION"]
["C14.1.2","Mobile access units"]
["C14.1.2.1","Establishment of mobile access unit on site (to reach a maximum height of 10m)","lump sum"]
["C14.1.2.2","Setting up of mobile access unit at each structure location and removal after completion","number (No.)"]
["C14.1.2.3","Operation of mobile access unit during repair work at each location (relevant elements of structure)","days"]
["C14.1.2.4","Operation of mobile access unit during inspections by the Engineer","hour (h)"]
["C14.1.2.5","De-establishing and removal of mobile access unit from site after completion of work","lump sum"]
["C14.1.4","Attendance by Rail Authority"]
["C14.1.4.1","Prime cost sum to allow for attendance by the relevant rail authority to obtain access near electrified railway lines or other relevant authorities as required at the repair site ","prime cost (PC) sum"]
["C14.1.4.2","Percentage on prime cost sum for charges and profits","percentage (%)"]
["PSC14.1.8","Temporary access scaffolding platform with minimum 5m² working area"]
["PSC14.1.8.1","Establishment of temporary access scaffolding platform on site"]
["PSC14.1.8.1(a)","For access between 0m and 6m in height"]
["PSC14.1.8.1(a)(i)","Deck","lump sum"]
["PSC14.1.8.1(a)(ii)","Pier","lump sum"]
["PSC14.1.8.1(a)(iiv)","Abutment","lump sum"]
["PSC14.1.8.1(a)(iv)","Walls","lump sum"]
["PSC14.1.8.1(a)(v)","Culvert barrel including headwall","lump sum"]
["PSC14.1.8.1(b)","For access between 6m and 10m in height"]
["PSC14.1.8.1(b)(i)","Deck","lump sum"]
["PSC14.1.8.1(b)(ii)","Pier","lump sum"]
["PSC14.1.8.1(b)(iiv)","Abutment","lump sum"]
["PSC14.1.8.1(b)(iv)","Walls","lump sum"]
["PSC14.1.8.1(b)(v)","Culvert barrel including headwall","lump sum"]
["PSC14.1.8.1(c)","For access greater than 10m in height"]
["PSC14.1.8.1(c)(i)","Deck","lump sum"]
["PSC14.1.8.1(c)(ii)","Pier","lump sum"]
["PSC14.1.8.1(c)(iiv)","Abutment","lump sum"]
["PSC14.1.8.1(c)(iv)","Walls","lump sum"]
["PSC14.1.8.1(c)(v)","Culvert barrel including headwall","lump sum"]
["PSC14.1.8.2","Setting up of temporary access scaffolding platform at each structure location and removal after completion"]
["PSC14.1.8.2(a)","For access between 0m and 6m in height"]
["PSC14.1.8.2(a)(i)","Deck","number (No.)"]
["PSC14.1.8.2(a)(ii)","Pier","number (No.)"]
["PSC14.1.8.2(a)(iiv)","Abutment","number (No.)"]
["PSC14.1.8.2(a)(iv)","Walls","number (No.)"]
["PSC14.1.8.2(a)(v)","Culvert barrel including headwall","number (No.)"]
["PSC14.1.8.2(b)","For access between 6m and 10m in height"]
["PSC14.1.8.2(b)(i)","Deck","number (No.)"]
["PSC14.1.8.2(b)(ii)","Pier","number (No.)"]
["PSC14.1.8.2(b)(iiv)","Abutment","number (No.)"]
["PSC14.1.8.2(b)(iv)","Walls","number (No.)"]
["PSC14.1.8.2(b)(v)","Culvert barrel including headwall","number (No.)"]
["PSC14.1.8.2(c)","For access greater than 10m in height"]
["PSC14.1.8.2(c)(i)","Deck","number (No.)"]
["PSC14.1.8.2(c)(ii)","Pier","number (No.)"]
["PSC14.1.8.2(c)(iiv)","Abutment","number (No.)"]
["PSC14.1.8.2(c)(iv)","Walls","number (No.)"]
["PSC14.1.8.2(c)(v)","Culvert barrel including headwall","number (No.)"]
["PSC14.1.8.3","Operation and maintenance of the temporary access scaffolding platform at each structure location "]
["PSC14.1.8.3(a)","For access between 0m and 6m in height"]
["PSC14.1.8.3(a)(i)","Deck","days"]
["PSC14.1.8.3(a)(ii)","Pier","days"]
["PSC14.1.8.3(a)(iiv)","Abutment","days"]
["PSC14.1.8.3(a)(iv)","Walls","days"]
["PSC14.1.8.3(a)(v)","Culvert barrel including headwall","days"]
["PSC14.1.8.3(b)","For access between 6m and 10m in height"]
["PSC14.1.8.3(b)(i)","Deck","days"]
["PSC14.1.8.3(b)(ii)","Pier","days"]
["PSC14.1.8.3(b)(iiv)","Abutment","days"]
["PSC14.1.8.3(b)(iv)","Walls","days"]
["PSC14.1.8.3(b)(v)","Culvert barrel including headwall","days"]
["PSC14.1.8.3(c)","For access greater than 10m in height"]
["PSC14.1.8.3(c)(i)","Deck","days"]
["PSC14.1.8.3(c)(ii)","Pier","days"]
["PSC14.1.8.3(c)(iiv)","Abutment","days"]
["PSC14.1.8.3(c)(iv)","Walls","days"]
["PSC14.1.8.3(c)(v)","Culvert barrel including headwall","days"]
["PSC14.1.8.4","De-establishing and removal of access scaffolding platform from site after completion of work"]
["PSC14.1.8.4(a)","For access between 0m and 6m in height"]
["PSC14.1.8.4(a)(i)","Deck","lump sum"]
["PSC14.1.8.4(a)(ii)","Pier","lump sum"]
["PSC14.1.8.4(a)(iiv)","Abutment","lump sum"]
["PSC14.1.8.4(a)(iv)","Walls","lump sum"]
["PSC14.1.8.4(a)(v)","Culvert barrel including headwall","lump sum"]
["PSC14.1.8.4(b)","For access between 6m and 10m in height"]
["PSC14.1.8.4(b)(i)","Deck","lump sum"]
["PSC14.1.8.4(b)(ii)","Pier","lump sum"]
["PSC14.1.8.4(b)(iiv)","Abutment","lump sum"]
["PSC14.1.8.4(b)(iv)","Walls","lump sum"]
["PSC14.1.8.4(b)(v)","Culvert barrel including headwall","lump sum"]
["PSC14.1.8.4(c)","For access greater than 10m in height"]
["PSC14.1.8.4(c)(i)","Deck","lump sum"]
["PSC14.1.8.4(c)(ii)","Pier","lump sum"]
["PSC14.1.8.4(c)(iiv)","Abutment","lump sum"]
["PSC14.1.8.4(c)(iv)","Walls","lump sum"]
["PSC14.1.8.4(c)(v)","Culvert barrel including headwall","lump sum"]
["PSC14.1.9","Suspended access platforms to deck "]
["PSC14.1.9.1","Establishment of suspended access platforms on site "]
["PSC14.1.9.1(a)","Deck sides or outside of parapets (5m² platform working area)","lump sum"]
["PSC14.1.9.1(b)","Deck soffit (10m² platform working area)","lump sum"]
["PSC14.1.9.2","Setting up of suspended access platform at each structure location and removal after completion"]
["PSC14.1.9.2(a)","Deck sides or outside of parapets (5m² platform working area)","number (No.)"]
["PSC14.1.9.2(b)","Deck soffit (10m² platform working area)","number (No.)"]
["PSC14.1.9.3","Operation and maintenance of suspended access platform at each structure location"]
["PSC14.1.9.3(a)","Deck sides or outside of parapets (5m² platform working area)","days"]
["PSC14.1.9.3(b)","Deck soffit (10m² platform working area)","days"]
["PSC14.1.9.4","De-establishing and removal of suspended access platform from site after completion of work"]
["PSC14.1.9.4(a)","Deck sides or outside of parapets (5m² platform working area)","lump sum"]
["PSC14.1.9.4(b)","Deck soffit (10m² platform working area)","lump sum"]
["CHAPTER 14: REPAIR OF STRUCTURES"]
["ITEM","DESCRIPTION","UNIT"]
["SECTION 14.2: CORROSION SURVEY METHODS AND TESTING OF NEAR SURFACE CONCRETE PROPERTIES"]
["C14.2.1","Delamination Survey:"]
["C14.2.1.1","Using hammer tapping technique to existing concrete members","square metre (m2)"]
["C14.2.2","Concrete cover survey "]
["C14.2.2.1","Existing concrete members on bridges","square metre (m2)"]
["C14.2.2.2","Existing concrete members on culverts","square metre (m2)"]
["CHAPTER 14: REPAIR OF STRUCTURES"]
["ITEM","DESCRIPTION","UNIT"]
["SECTION 14.3: DEMOLITION AND REMOVAL OF STRUCTURAL CONCRETE AND STEELWORK"]
["C14.3.1","Demolition of concrete members or elements "]
["C14.3.1.2","Partial member or element (location and description)"]
["C14.3.1.2(a)","Abutments","cubic metre (m3)"]
["C14.3.1.2(b)","Piers","cubic metre (m3)"]
["C14.3.1.2(c) ","Walls","cubic metre (m3)"]
["C14.3.1.2(d)","Parapets including enbdlock","cubic metre (m3)"]
["C14.3.1.2(e)","Deck longitudinal members","cubic metre (m3)"]
["C14.3.1.2(f)","Deck transverse members","cubic metre (m3)"]
["C14.3.1.2(g) ","Deck slabs","cubic metre (m3)"]
["C14.3.1.2(h)","Foundations","cubic metre (m3)"]
["C14.3.3","Demolition of structural steel structures, members or elements (location and description)"]
["C14.3.3.2","Partial member or element (location and description)"]
["C14.3.3.2(a)","Steelwork","ton (t)"]
["C14.3.5","Removal of metal sections embedded in concrete (description)"]
["C14.3.5.1","Handrail posts embedded in concrete (pocket size of 120 x 120 x 50mm)","number (No.)"]
["C14.3.5.2","Handrail posts embedded concrete (pocket sizes of 150 x 150 x 50mm)","number (No.)"]
["C14.3.5.3","Grinding exposed stubs of removed handrail posts flush with top of concrete","number (No.)"]
["C14.3.5.4","Cut back tie rods and make good (pocket size 50 x 50 x 50mm)","number (No.)"]
["C14.3.5.5","Cut back or removal of embedded reinforcement and make good (pocket size of 50 x 50 x 50mm)","number (No.)"]
["CHAPTER 14: REPAIR OF STRUCTURES"]
["ITEM","DESCRIPTION","UNIT"]
["SECTION 14.4: SURFACE AND STRUCTURAL REPAIR OF CONCRETE MEMBERS"]
["PSC14.4.3","Proprietary cementitious repair system in accordance with Table A14.4.5-1"]
["PSC14.4.3.1","Class R4 cement-based, shrinkage compensated, low permeablility repair mortar that is suitable for Principle 3, Method 3.1 of EN1504 for hand applied mortar to positions as indicated:"]
["PSC14.4.3.1(a)","Concrete handrails posts and top rails","litre (ℓ)"]
["PSC14.4.3.1(b)","Conrete at joint turnups on parapets","litre (ℓ)"]
["PSC14.4.3.1(c)","Honeycombed concrete on abutments","litre (ℓ)"]
["PSC14.4.3.1(d)","Honeycombed concrete on piers","litre (ℓ)"]
["PSC14.4.3.1(e)","Honeycombed concrete on walls","litre (ℓ)"]
["PSC14.4.3.1(f)","Honeycombed concrete on parapets","litre (ℓ)"]
["PSC14.4.3.1(g)","Honeycombed concrete on deck longitudinal members","litre (ℓ)"]
["PSC14.4.3.1(h)","Honeycombed concrete on deck transverse members","litre (ℓ)"]
["PSC14.4.3.1(i)","Honeycombed concrete on deck slabs","litre (ℓ)"]
["PSC14.4.3.1(j)","Honeycombed concrete on foundations","litre (ℓ)"]
["PSC14.4.3.1(k)","Spalled concrete on abutments","litre (ℓ)"]
["PSC14.4.3.1(l)","Spalled concrete on piers","litre (ℓ)"]
["PSC14.4.3.1(m)","Spalled concrete on walls","litre (ℓ)"]
["PSC14.4.3.1(n)","Spalled concrete on parapets","litre (ℓ)"]
["PSC14.4.3.1(o)","Spalled concrete on deck longitudinal members","litre (ℓ)"]
["PSC14.4.3.1(p)","Spalled concrete on deck transverse members","litre (ℓ)"]
["PSC14.4.3.1(q)","Spalled concrete on deck slabs","litre (ℓ)"]
["PSC14.4.3.1(r)","Spalled concrete on foundations","litre (ℓ)"]
["PSC14.4.3.2","Class R4, self compacting, shrinkage compensated, microconcrete that is suitable for Principle 3, Method 3.2 of EN 1504-9 for recasting with concrete or mortar to positions as indicated:"]
["PSC14.4.3.2(a)","Abutments","litre (ℓ)"]
["PSC14.4.3.2(b)","Piers","litre (ℓ)"]
["PSC14.4.3.2(c)","Walls","litre (ℓ)"]
["PSC14.4.3.2(d)","Parapets including endblocks","litre (ℓ)"]
["PSC14.4.3.2(e)","Deck longitudinal members","litre (ℓ)"]
["PSC14.4.3.2(f)","Deck transverse members","litre (ℓ)"]
["PSC14.4.3.2(g)","Deck slabs","litre (ℓ)"]
["PSC14.4.3.2(h)","Foundations","litre (ℓ)"]
["PSC14.4.3.2(i)","Sidewalks","litre (ℓ)"]
["PSC14.4.3.2(j)","Culvert barrel","litre (ℓ)"]
["PSC14.4.3.2(k)","Culvert headwall","litre (ℓ)"]
["PSC14.4.3.2(l)","Apron slabs and cut off walls","litre (ℓ)"]
["CHAPTER 14: REPAIR OF STRUCTURES"]
["ITEM","DESCRIPTION","UNIT"]
["SECTION 14.5: ANCHORING OF REINFORCEMENT, GROUTING AND CRACK INJECTION"]
["C14.5.1","Anchoring of reinforcing steel:"]
["C14.5.1.1","Reinforcing (type, bar diameter) into formed holes (hole diameter and depth stated) in (description of member) "]
["C14.5.1.1(a)","Reinforcing (Y10 bars) into formed holes (15mm hole diameter, 150mm hole depth) in existing concrete","number (No.)"]
["C14.5.1.1(b)","Reinforcing (Y12 bars) into formed holes (18mm hole diameter, 180mm hole depth) in existing concrete","number (No.)"]
["C14.5.1.1(c)","Reinforcing (Y16 bars) into formed holes (24mm hole diameter, 240mm hole depth) in existing concrete","number (No.)"]
["C14.5.1.1(d)","Reinforcing (Y20 bars) into formed holes (30mm hole diameter, 300mm hole depth) in existing concrete","number (No.)"]
["C14.5.1.1(e)","Reinforcing (Y25 bars) into formed holes (38mm hole diameter, 375mm hole depth) in existing concrete","number (No.)"]
["C14.5.2","Preparation of contact surfaces for grouting (preparation of 1m² of concrete parapet surface for installation of precast top rail)","number (No.)"]
["C14.5.3","Grouting for"]
["C14.5.3.1","Bedding (grouting underneath precast concrete parapets)","litre (ℓ)"]
["C14.5.3.2","Gap filling (filling pockets or holes)","litre (ℓ)"]
["C14.5.4","Establishment on site for crack injection","lump sum"]
["C14.5.5","Surface preparation and surface sealing for crack injection to (location on structure)"]
["C14.5.5.1","Abutments","metre (m)"]
["C14.5.5.2","Piers","metre (m)"]
["C14.5.5.3","Walls","metre (m)"]
["C14.5.5.4","Parapets","metre (m)"]
["C14.5.5.5","Deck","metre (m)"]
["C14.5.5.6","Culvert barrel","metre (m)"]
["C14.5.5.7","Culvert headwall","metre (m)"]
["C14.5.6","Crack injection adhesive to (location on structure)"]
["C14.5.6.1","Abutments","litre (ℓ)"]
["C14.5.6.2","Piers","litre (ℓ)"]
["C14.5.6.3","Walls","litre (ℓ)"]
["C14.5.6.4","Parapets","litre (ℓ)"]
["C14.5.6.5","Deck","litre (ℓ)"]
["C14.5.6.6","Culvert barrel","litre (ℓ)"]
["C14.5.6.7","Culvert headwall","litre (ℓ)"]
["C14.5.7","Crack filling "]
["C14.5.7.1","Repair system to (location on structure)"]
["C14.5.7.1(a)","Abutments","metre (m)"]
["C14.5.7.1(b)","Piers","metre (m)"]
["C14.5.7.1(c)","Walls","metre (m)"]
["C14.5.7.1(d)","Parapets","metre (m)"]
["C14.5.7.1(e)","Deck","metre (m)"]
["C14.5.7.1(f)","Culvert barrel","metre (m)"]
["C14.5.7.1(g)","Culvert headwall","metre (m)"]
["CHAPTER 14: REPAIR OF STRUCTURES"]
["ITEM","DESCRIPTION","UNIT"]
["SECTION 14.7: PROTECTIVE COATINGS AND TREATMENTS FOR CONCRETE"]
["C14.7.1","Cleaning and preparation of concrete surface"]
["C14.7.1.1","Hand scrubbing with water and detergent (to remove curing compounds or membranes, shutter release compounds, corrosion stains, and water-soluble contaminants without inadvertently damaging the concrete appearance and without producing an exposed aggregate finish)","square metre (m2)"]
["C14.7.1.2","High-pressure water-jetting (to remove curing compounds or membranes, shutter release compounds, corrosion stains, and water-soluble contaminants without inadvertently damaging the concrete appearance and without producing an exposed aggregate finish)","square metre (m2)"]
["PSC14.7.2","Application of protective coatings and treatments in accordance with A14.7.5"]
["PSC14.7.2.1","Hydrophobic impregnants","square metre (m2)"]
["PSC14.7.2.2","Sealers and pore blockers","square metre (m2)"]
["PSC14.7.2.3","Coatings"]
["PSC14.7.2.3a","Two coats of Sikalastic 152 or equivalent to exposed concrete surfaces.","square metre (m2)"]
["PSC14.7.2.3b","Application of protective coatings that includes 1 coat of Primer with 2 coats of Sikagard 550W Elastic or equivalent to all concrete surfaces.","square metre (m2)"]
["PSC14.7.2.4","Renderings","square metre (m2)"]
["PSC14.7.2.5","Corrosion inhibitor"]
["PSC14.7.2.5a","Application of Corrosion inhibitor Sika Ferroguard 903 or equivalent to all concrete repair sections","square metre (m2)"]
["PSC14.7.2.5b","Application of Sika Armatec 110 EC or equivalent to all concrete surface areas exposed for repairs and all exposed reinforced steel","square metre (m2)"]
["C14.7.4","Trial sample panels"]
["C14.7.4.1","Hydrophobic impregnants","square metre (m2)"]
["C14.7.4.2","Sealers and pore blockers","square metre (m2)"]
["C14.7.4.3","Coatings","square metre (m2)"]
["C14.7.4.4","Renderings","square metre (m2)"]
["C14.7.4.5","Corrosion inhibitor","square metre (m2)"]
["CHAPTER 14: REPAIR OF STRUCTURES"]
["ITEM","DESCRIPTION","UNIT"]
["SECTION 14.9: REPAIR AND REPLACEMENT OF ANCILLARY STRUCTURAL ELEMENTS"]
["C14.9.2","Clear bridge drainage system (description of elements)"]
["C14.9.2.1","Scuppers","number (No.)"]
["C14.9.2.2","Weepholes","number (No.)"]
["C14.9.2.3","Drainage pipes","number (No.)"]
["PSC14.9.3","Service and repair of existing joint system"]
["PSC14.9.3.1","Cleaning of existing joint grooves","metre (m)"]
["PSC14.9.3.2","Replacement of existing glands in claw type joints up to 80mm wide","metre (m)"]
["PSC14.9.3.3","Refurbishment of existing steel edging in joint, including removal of surface rust and application of a corrosion protection system 6 (COTO section PSA13.12.7.15) or similar approved","square metre (m2)"]
["PSC14.9.3.4","Complete removal and replacement of existing concrete nosing in 40mm claw type joints","litre (ℓ)"]
["PSC14.9.3.5","Complete removal and replacement of existing concrete nosing in 80mm claw type joints","litre (ℓ)"]
["PSC14.9.3.6","Tightening of nuts and bolts","Number (No.)"]
["PSC14.9.3.7","Complete removal and disposal of existing asphaltic plug joint - up to 500 x 100mm","metre (m)"]
["PSC14.9.3.8","Complete removal and disposal of existing 40mm claw joint","metre (m)"]
["PSC14.9.3.9","Complete removal and disposal of existing 80mm claw joint","metre (m)"]
["PSC14.9.3.10","Complete removal and disposal of compression seal type joints up to 40mm wide","metre (m)"]
["PSC14.9.3.11","Complete removal, disposal and replacement of field poured sealant type joints (silicone sealant with backing cord) of up to 20 x 20mm in size","metre (m)"]
["C14.9.4","Joint terminations as specified on the drawings in:"]
["C14.9.4.1","Barriers and Parapets (claw type joint)","number (No.)"]
["C14.9.4.2","Sidewalks (claw type joint)","number (No.)"]
["C14.9.5","Cover plates (non-metallic) in barriers, parapets and sidewalks as specified on the drawings in:"]
["C14.9.5.1","Barriers and parapets"]
["C14.9.5.1(a)","Cover plate on parapets at joint termination (detail S5023-5009)","number (No.)"]
["C14.9.5.1(b)","Service duct cover on parapets (300 x 150mm)","number (No.)"]
["C14.9.5.2","Sidewalks"]
["C14.9.5.2(a)","Cover plate on sidewalks at joint termination (detail S5023-5009)","number (No.)"]
["C14.9.5.2(b)","Service duct cover on sidewalks (300 x 150mm)","number (No.)"]
["PSC14.9.6","Repair of handrails (repair, realignment, reinstallation, or refixing of existing steel handrails)","metre (m)"]
["PSC14.9.7","Removal and reinstatement of brickwork "]
["PSC14.9.7.1","Removal of brickwork","cubic metre (m3)"]
["PSC14.9.7.2","Reinstating or newly constructed brickwork","cubic metre (m3)"]
["C14.9.8","Drilling of drainage holes into void formers from deck soffit (up to 100mm dia.)","number (No.)"]
["PSC14.9.9","Refurbishment of bearings "]
["PSC14.9.9.1","In-situ bearing refurbishment (including removal of surface rust and application of a paint system - System 6 in COTO section PSA13.12.7.15 or similar approved)","square metre (m2)"]
["PSC14.9.9.2","In-situ repair of bearing plinths","litre (ℓ)"]
["C14.9.10","Replace PVC junctions in deck (type and size described)"]
["C14.9.10.1","110mm","number (No.)"]
["C14.9.10.2","150mm","number (No.)"]
["C14.9.16","Supply new ancillary elements"]
["C14.9.16.1","Extend scuppers below deck soffit"]
["C14.9.16.1(a)","Up to 100mm diameter","metre (m)"]
["C14.9.16.1(b)","Greater than 100mm in diameter","metre (m)"]
["PSC14.9.18","Install new drain pipe to bearing shelf (up to 100mm dia.)","metre (m)"]
["CHAPTER 14: REPAIR OF STRUCTURES"]
["ITEM","DESCRIPTION","UNIT"]
["SECTION 14.10: JACKING OF BRIDGE STRUCTURES"]
["PSC14.10.1","Temporary support and foundations"]
["PSC14.10.1.1","Design, construct and erect temporary supports for the jacking of a bridge deck with a capacity at a support as indicated:"]
["PSC14.10.1.1(a)","50 tonnes","number (No.)"]
["PSC14.10.1.1(b)","100 tonnes","number (No.)"]
["PSC14.10.1.2","Dismantle and remove from site all temporary supports with a capacity at a support as indicated:"]
["PSC14.10.1.2(a)","50 tonnes","number (No.)"]
["PSC14.10.1.2(b)","100 tonnes","number (No.)"]
["PSC14.10.2","Jacking equipment"]
["PSC14.10.2.1","Design, supply and install equipment for the jacking of a bridge deck  with a capacity as indicated:"]
["PSC14.10.2.1(a)","50 tonnes","number (No.)"]
["PSC14.10.2.1(b)","100 tonnes","number (No.)"]
["PSC14.10.2.2","Dismantle and remove all jacking equipment from site with a capacity as indicated:"]
["PSC14.10.2.2(a)","50 tonnes","number (No.)"]
["PSC14.10.2.2(b)","100 tonnes","number (No.)"]
["PSC14.10.3","Vertical jacking of the bridge deck ","tonnes (t)"]
["CHAPTER 14: REPAIR OF STRUCTURES"]
["ITEM","DESCRIPTION","UNIT"]
["SECTION 14.11: REPAIR OF STEEL ELEMENTS"]
["C14.11.2","Replacement of rivets or bolts with HSFG bolts (diameter and class indicated)"]
["C14.11.2.1","Class 4.8 bolts"]
["C14.11.2.1(a)","M12","number (No.)"]
["C14.11.2.1(b)","M16","number (No.)"]
["C14.11.2.1(c) ","M20","number (No.)"]
["C14.11.2.1(d)","M24","number (No.)"]
["C14.11.2.1(e)","M30","number (No.)"]
["C14.11.2.1(f)","M36","number (No.)"]
["C14.11.2.2","Class 8.8 bolts"]
["C14.11.2.2(b)","M16","number (No.)"]
["C14.11.2.2(c) ","M20","number (No.)"]
["C14.11.2.2(d)","M24","number (No.)"]
["C14.11.2.2(e)","M30","number (No.)"]
["C14.11.2.2(f)","M36","number (No.)"]
["C14.11.2.3","Class 10.9 bolts"]
["C14.11.2.3(b)","M16","number (No.)"]
["C14.11.2.3(c) ","M20","number (No.)"]
["C14.11.2.3(d)","M24","number (No.)"]
["C14.11.2.3(e)","M30","number (No.)"]
["C14.11.2.3(f)","M36","number (No.)"]
["PSC14.11.3","Removal of damaged or corroded steel members and replacement with new members"]
["PSC14.11.3.1","Removal of damaged or corroded steel members ","kilogram (kg)"]
["PSC14.11.3.2","New replacement steel members including installation","kilogram (kg)"]
["PSC14.11.4","Removal and replacement of roof sheeting on closed bridge walkways"]
["PSC14.11.4.1","Type and thickness of sheeting as indicated"]
["PSC14.11.4.1(a)","Steel IBR roof sheeting (galvanised and painted)"]
["PSC14.11.4.1(a)(i)","0.40mm thick","square metre (m2)"]
["PSC14.11.4.1(a)(ii)","0.48mm thick","square metre (m2)"]
["PSC14.11.4.1(a)(iii)","0.50mm thick","square metre (m2)"]
["PSC14.11.4.1(a)(iv)","0.55mm thick","square metre (m2)"]
["PSC14.11.4.1(a)(v)","0.58mm thick","square metre (m2)"]
["PSC14.11.4.1(a)(vi)","0.80mm thick","square metre (m2)"]
["PSC14.11.4.1(b)","Steel corrugated roof sheeting (galvanised and painted)"]
["PSC14.11.4.1(b)(i)","0.40mm thick","square metre (m2)"]
["PSC14.11.4.1(b)(ii)","0.48mm thick","square metre (m2)"]
["PSC14.11.4.1(b)(iii)","0.50mm thick","square metre (m2)"]
["PSC14.11.4.1(b)(iv)","0.55mm thick","square metre (m2)"]
["PSC14.11.4.1(b)(v)","0.58mm thick","square metre (m2)"]
["PSC14.11.4.1(b)(vi)","0.80mm thick","square metre (m2)"]
["PSC14.11.4.2","Provision for other types of sheeting","provisional sum"]
["PSC14.11.4.3","Handling cost, profit and all other charges in respect of item PSC14.11.4.2","percentage (%)"]
["PSC14.11.5","Re-torquing of bolts on structural steel"]
["PSC14.11.5.1","Bolts up to and including 8mm in diameter","number (No.)"]
["PSC14.11.5.2","Bolts from 12mm to 20mm in diameter","number (No.)"]
["PSC14.11.5.3","Bolts from 20mm to 36mm in diameter","number (No.)"]
["PSC14.11.6","Welding"]
["PSC14.11.6.1","6mm fillet weld","metre (m)"]
["CHAPTER 20: QAULITY ASSURANCE"]
["ITEM","DESCRIPTION","UNIT"]
["SECTION 20.1: TESTING MATERIALS AND JUDGEMENT OF WORKMANSHIP"]
["PSC20.1.6","Provision for commercial laboratory testing"]
["PSC20.1.6(a)","Actual cost of testing","Prov sum"]
["PSC20.1.6(b)","Contractor's charges in respect of subitem C20.1.6(a) above","%"]

{"sheet":"Category B","index":1,"n_rows":1224,"n_cols":18,"rows_kept":1224,"cut":false,"hidden":false,"merged":[]}
["C2.2 SCHEDULE OF RATES ","CATEGORY B - TERM TENDER FOR ROAD STRUCTURES AND ANCILLARY WORKS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["CHAPTER 1: GENERAL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["ITEM","DESCRIPTION","UNIT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["SECTION 1.2: GENERAL REQUIREMENTS AND PROVISIONS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.2.1","Environmental Management",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.2.1.1","Monitoring of compliance with and reporting on the EMP","day"]
["PSC1.2.1.3","Environmental Emergency Measures"]
["PSC1.2.1.3(a)","Provision of environmental emergency measures","PC Sum"]
["PSC1.2.1.3(b)","Contractor's charge to allow for handling costs and profit in respect of subitem PSC1.2.1.3(a) ","percentage (%)"]
["PSC1.2.1.4","Penalty to be deducted for non-compliance with requirements of Environmental management"]
["PSC1.2.1.4(a)","Vehicles, plant or materials related to the Contractor’s operations, parked or stored outside the demarcated boundaries of the Site","Number (No)"]
["PSC1.2.1.4(b)","Persons, vehicles, plant or materials related to the Contractor’s operations, found within the designated boundaries of a “no go” area","Number (No)"]
["PSC1.2.1.4 (c)","Persistent and unrepaired oil leaks from machinery/not using a drip tray to collect waste oil and other lubricants/not using specified absorbent material to encapsulate hydrocarbon spillage/using inappropriate methods of refuelling (the use of a funnel rather than a pump). ","Number (No)"]
["PSC1.2.1.4 (d)","Refuelling in areas not approved by the Employer’s Agent. ","Number (No)"]
["PSC1.2.1.4(e)","Waste and Litter on Site.","Number (No)"]
["PSC1.2.1.4(f)","Deliberate lighting of fires on Site.  ","Number (No)"]
["PSC1.2.1.4(g)","Individual not making use of the Site ablution facilities. ","Number (No)"]
["PSC1.2.1.4(h)","Damage to trees not specified to be removed. ","Number (No)"]
["PSC1.2.1.4(i)","Dust or excessive noise emanating from the site ","Number (No)"]
["PSC1.2.1.4 (j)","Damage or pollution of wetlands, rivers and surrounding areas","Number (No)"]
["PSC1.2.2","Programming and Reporting"]
["PSC1.2.2.1","Submission of a Scheme 1 Programme","lump sum"]
["PSC1.2.4","Stakeholder liaison"]
["PSC1.2.4.1","Remuneration of Community Liaison Officer (CLO) (as per CCT published rate. CPA will apply if rate is revised)                         ","day"]
["PSC1.2.4.2","Contractor’s charge to allow for handling costs and profit in respect of subitem PSC1.2.4.1            ","percentage (%)"]
["PSC1.2.5","Safety "]
["C1.2.5.1","Health and safety plan","lump sum"]
["PSC1.2.5.2","Implementation of health and safety plan","day"]
["PSC1.2.8","Dayworks"]
["PSC1.2.8.1","Personnel"]
["PSC1.2.8.1(a)","Unskilled labourer","hour (h)"]
["PSC1.2.8.1(b)","Semi-skilled labourer","hour (h)"]
["PSC1.2.8.1(c)","Skilled labourer","hour (h)"]
["PSC1.2.8.1(d)","Gang leader","hour (h)"]
["PSC1.2.8.1(e)","Foreman","hour (h)"]
["PSC1.2.8.1(f)","Skilled artisan","hour (h)"]
["PSC1.2.8.1(g)","Welder (in accordance with welder qualification requirements of A13.11.8.1(b))","hour (h)"]
["PSC1.2.8.2","Construction equipment"]
["PSC1.2.8.2(a)","Tractor loader backhoe (55kW)","hour (h)"]
["PSC1.2.8.2(b)","Generator","hour (h)"]
["PSC1.2.8.2(c)","Compressor","hour (h)"]
["PSC1.2.8.2(d)","Welding machine (500A)","hour (h)"]
["PSC1.2.8.2(e)","Other Plant/Equipment not specified above"]
["PSC1.2.8.2(e)(i)","Procurement of plant/equipment- actual cost of plant/equipment not already specified in the tender by the employer","provisional sum"]
["PSC1.2.8.2(e)(ii)","Handling cost, profit and all other charges in respect of item PSC1.2.8.2(h)(i)","percentage (%)"]
["C1.2.8.3","Vehicles "]
["C1.2.8.3(a)","Light delivery vehicle (1 tonne)","kilometre (km)"]
["C1.2.8.3(b)","Flatbed truck (with crane capable of transporting and placing/removing concrete new jersey type barriers)","kilometre (km)"]
["C1.2.8.3(c)","Dump truck (6m³)","kilometre (km)"]
["C1.2.8.4","Materials"]
["C1.2.8.4(a)","Procurement of materials","provisional sum"]
["C1.2.8.4(b)","Contractor's handling costs, profit and all other charges in respect of item C1.2.8.4(a)","percentage (%)"]
["PSC1.2.10","Dispute Adjudication Board (DAB)"]
["PSC1.2.10.1","Employer’s contribution to DAB (50%)","PC Sum"]
["CHAPTER 1: GENERAL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["ITEM","DESCRIPTION","UNIT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["SECTION 1.3: CONTRACTOR’S ESTABLISHMENT ON SITE AND GENERAL OBLIGATIONS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.3.1","The Contractor's general obligations",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.3.1.1","The Contractor’s general obligations for Work Projects greater than R3 000 001 up to and including R3 500 000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.3.1.1(a)","Fixed obligations","lump sum",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.3.1.1(b)","Time-related obligations","day",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.3.1.1(c)","Extra-over sub-items (a) and (b) for working on designated non-working and special non-working days as instructed by the Employer","day",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.3.1.2","The Contractor’s general obligations for Work Projects greater than R3 500 001 up to and including R4 000 000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.3.1.2(a)","Fixed obligations","lump sum",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.3.1.2(b)","Time-related obligations","day",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.3.1.2(c)","Extra-over sub-items (a) and (b) for working on designated non-working and special non-working days as instructed by the Employer","day",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.3.1.3","The Contractor’s general obligations for Work Projects greater than R4 000 001 up to and including R4 500 000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.3.1.3(a)","Fixed obligations","lump sum",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.3.1.3(b)","Time-related obligations","day",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.3.1.3(c)","Extra-over sub-items (a) and (b) for working on designated non-working and special non-working days as instructed by the Employer","day",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.3.1.4","The Contractor’s general obligations for Work Projects greater than R4 500 001 up to and including R5 000 000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.3.1.4(a)","Fixed obligations","lump sum",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.3.1.4(b)","Time-related obligations","day",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.3.1.4(c)","Extra-over sub-items (a) and (b) for working on designated non-working and special non-working days as instructed by the Employer","day",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.3.1.5","The Contractor’s general obligations for Work Projects greater than R5 500 001 up to and including R5 500 000"]
["PSC1.3.1.5(a)","Fixed obligations","lump sum"]
["PSC1.3.1.5(b)","Time-related obligations","day"]
["PSC1.3.1.5(c)","Extra-over sub-items (a) and (b) for working on designated non-working and special non-working days as instructed by the Employer","day"]
["PSC1.3.1.6","The Contractor’s general obligations for Work Projects greater than R5 500 001 up to and including R6 000 000"]
["PSC1.3.1.6(a)","Fixed obligations","lump sum"]
["PSC1.3.1.6(b)","Time-related obligations","day"]
["PSC1.3.1.6(c)","Extra-over sub-items (a) and (b) for working on designated non-working and special non-working days as instructed by the Employer","day"]
["C1.3.2","Contract sign boards","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["CHAPTER 1: GENERAL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["ITEM","DESCRIPTION","UNIT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["SECTION 1.5: ACCOMMODATION OF TRAFFIC",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.5.1","Accommodation of pedestrian and non-motorised traffic",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.5.1.1","Accommodation of pedestrian and non-motorised traffic","day",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.5.2","Accommodation of vehicular traffic",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.5.2.1","Class 1: principal arterial (40 000 < vpd < 120 000)","day",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.5.2.2","Class 2: major arterial (20 000 < vpd < 60 000)","day",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.5.2.3","Class 3: minor arterial (10 000 < vpd < 40 000)","day",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.5.2.4","Class 4a: collector street, commercial (vpd < 25 000)","day",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.5.2.5","Class 4b: collector street, residential (vpd < 15 000)","day",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.5.2.6","Class 5a: local street, commercial (vpd < 5 000)","day",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.5.7","Temporary traffic control facilities",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5.7.1","Delineators including mounting bases and ballast:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5.7.1(a)","Single sided, reversible left or right (200 x 800mm)","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5.7.1(b)","Double sided, reversible left or right (200 x 800mm)","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5.7.2","Traffic cones, minimum height 750mm","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5.7.3","Flagmen","man-shift",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5.7.4","Traffic controllers","man-shift",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5.7.5","Provision of illuminated traffic signs:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5.7.5(a)","Sign mounted flashing amber lights (2 lights with the specified power supply) \nmounted on abacking board which is:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5.7.5(a)(i)","900mm wide x 150mm high","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5.7.5(a)(ii)","1200mm wide x 200mm high","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5.7.5(b)","Flashing LED illuminated arrow board","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.5.7.8","Traffic control stations","day",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.5.7.9","Cleaning of traffic control facilities","day",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.5.7.10","Barriers manufactured from plastic and ballasted with sand or water","metre (m)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.5.8","Traffic safety officer","man-shift",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.5.9","Traffic safety vehicle","day",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5.12","Additional traffic accommodation facilities ordered by the Engineer:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5.12.1","Provision of additional traffic accommodation facilities ","provisional sum",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5.12.2","Handling cost, profit and all other charges in respect of item C1.5.12.1","percentage (%)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.5.13","Penalty to be deducted for non-compliance with requirements for accommodation of traffic",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.5.13.1","Fixed penalty per occurrence","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.5.13.2","Time-related penalty","hour (hr)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5 / C11.4.2","Performance based vehicle restraint systems",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5/C11.4.2.1","Complete longitudinal barrier system to EN 1317 or AASHTO MASH or NCHRP350 as alternative where no MASH product is available:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5/11.4.2.1(c)","Concrete barrier system (H1, W4 according to EN1317 or MASH equivalent)","metre (m)"]
["C1.5/11.4.2.2","Terminal sections for the following to EN 1317 or AASHTO MASH or NCHRP350 as alternative where no MASH product is available:"]
["C1.5/11.4.2.2(a)","End treatments (Test Level 80/1 according to EN1317-3 or MASH equivalent)","number (No.)"]
["C1.5/11.4.2.3","Relocation of temporary systems (H1, W4 according to EN1317 or MASH equivalent)","metre (m)"]
["C1.5/C11.6.1.8","Regulatory signs, temporary (TR-series)"]
["C1.5/C11.6.1.8(a)","600mm size ","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5/C11.6.1.8(b)","900mm size ","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5/C11.6.1.8(c)","1200mm size ","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5/C11.6.1.10","Warning signs, temporary (TW-series) ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5/C11.6.1.10(a)","600mm size ","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5/C11.6.1.10(b)","900mm size ","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5/C11.6.1.10(c)","1200mm size ","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5/C11.6.1.10(d)","1500mm size ","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5/PSC11.6.1.13","Portable STOP and GO-RY signs","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.5/PSC11.6.1.14","Other temporary standard road signs not specified above (STW-/DTG-/TGS-/TG-/TIN-series)","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["CHAPTER 1: GENERAL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["ITEM","DESCRIPTION","UNIT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["SECTION 1.6: CLEARING AND GRUBBING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC1.6.1","Clearing"]
["PSC1.6.1.1","Clearing with machines and some hand labour where necessary","square metre (m2)"]
["PSC1.6.1.2","Clearing with hand labour only when labour enhanced work is specified","square metre (m2)"]
["PSC1.6.2","Grubbing"]
["PSC1.6.2.1","Grubbing with machines and some hand labour where necessary","square metre (m2)"]
["PSC1.6.2.2","Grubbing with hand labour when labour enhancement work is specified or it is not practical to use a machine","square metre (m2)"]
["C1.6.3","Removal and grubbing of large trees and tree stumps:"]
["C1.6.3.1","Girth equal to or exceeding 1,0m up to and including 2,0m","number (No.)"]
["C1.6.3.2","Girth exceeding 2,0m up to and including 3,0m","number (No.)"]
["C1.6.3.3","Girth exceeding 3,0m","number (No.)"]
["CHAPTER 1: GENERAL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["ITEM","DESCRIPTION","UNIT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["SECTION 1.7: LOADING AND HAULING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C1.7.2","Hauling"]
["C1.7.2.2","Hauling material to spoil and off-loading it at a designated spoil or stockpile area:"]
["C1.7.2.2(a)","Cleared and grubbed material (organic matter and all other unsuitable or waste material)","cubic metre kilometre (m3.km)"]
["C1.7.2.2(b)","Soil and gravel material","cubic metre kilometre (m3.km)"]
["C1.7.2.2(c)","Boulders, hard material and concrete","cubic metre kilometre (m3.km)"]
["CHAPTER 2: SERVICES",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["ITEM","DESCRIPTION","UNIT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["SECTION 2.1: GENERAL REQUIREMENTS AND TRENCHING FOR SERVICES",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C2.1.1","Location, identification, protection and relocation of existing services"]
["C2.1.1.2","Permanent services relocation or protection work by others","PC Sum"]
["C2.1.1.3","Handling costs and profit in respect of item C2.1.1.2 above","percentage (%)"]
["CHAPTER 3: DRAINAGE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["ITEM","DESCRIPTION","UNIT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["SECTION 3.1: DRAINS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C3.1.2","Clearing, shaping and disposal of accumulated sediment in existing unlined open drains "]
["C3.1.2.1","Using conventional methods","cubic metre (m3)"]
["C3.1.2.2","Using labour enhanced construction methods","cubic metre (m3)"]
["C3.1.3","Excavation, clearing and disposal of accumulated sediment in existing lined drains and drainage systems"]
["C3.1.3.1","Using conventional methods (up to 1,5m):"]
["C3.1.3.1(a)","Manholes and inlet and outlet structures","cubic metre (m3)"]
["C3.1.3.1(b)","Culvert barrels","cubic metre (m3)"]
["C3.1.3.1(c)","Concrete or other lined side drains","cubic metre (m3)"]
["C3.1.3.2","Using conventional methods (in excess of 1,5m):"]
["C3.1.3.2(a)","Manholes and inlet and outlet structures","cubic metre (m3)"]
["C3.1.3.2(b)","Culvert barrels","cubic metre (m3)"]
["C3.1.3.2(c)","Concrete or other lined side drains","cubic metre (m3)"]
["C3.1.3.3","Using labour enhanced construction methods:"]
["C3.1.3.3(a)","Manholes and inlet and outlet structures","cubic metre (m3)"]
["C3.1.3.3(b)","Culvert barrels","cubic metre (m3)"]
["C3.1.3.3(c)","Concrete or other lined side drains","cubic metre (m3)"]
[]
["CHAPTER 3: DRAINAGE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["ITEM","DESCRIPTION","UNIT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["SECTION 3.3: CONCRETE KERBING AND CHANNELING, ASPHALT BERMS, CHUTES, DOWNPIPES, AS WELL AS CONCRETE, STONE PITCHED AND GABION LININGS FOR OPEN DRAINS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC3.3.1","Concrete kerbing:"]
["C3.3.1.1","Prefabricated kerbing"]
["C3.3.1.1(a)","E3 Edging (see Drawing No. RD1.3)"]
["C3.3.1.1(a)(i)","300mm units","metre (m)"]
["C3.3.1.1(a)(ii)","1000mm units","metre (m)"]
["C3.3.1.1(b)","E1 Edging (see Drawing No. RD1.3)"]
["C3.3.1.1(b)(i)","300mm units","metre (m)"]
["C3.3.1.1(b)(ii)","1000mm units","metre (m)"]
["C3.3.1.2","Cast in situ kerbing "]
["C3.3.1.2(a)","Transition kerb (BK2 to MK10) (RD1.1 to RD1.2)"]
["C3.3.1.2(a)(i)","1000mm units","metre (m)"]
["PSC3.3.1.3","Concrete channelling:"]
["PSC3.3.1.3(a)","Precast half round channel (see Drawing No. RD1.7)"]
["PSC3.3.1.3(a)(i)","Type W1","metre (m)"]
["PSC3.3.1.3(a)(ii)","Type W2","metre (m)"]
["PSC3.3.1.3(a)(iii)","Type W3","metre (m)"]
["PSC3.3.1.3(b)","Triple flat channel (2 No x C1 Channels plus 1 No C2 channel) (See drawing No RD1.4)","metre (m)"]
["PSC3.3.1.4","Extra over for item PSC3.3.1.3(b), for in-situ Concrete infill "]
["PSC3.3.1.4(a)","Cast in-situ 50mm width","metre (m)"]
["PSC3.3.1.4(b)","Cast in-situ 75mm width","metre (m)"]
["PSC3.3.1.4(c)","Cast in-situ 100mm width","metre (m)"]
["C3.3.5","Asphalt berms"]
["C3.3.5.1","Asphalt berms placed where there are no vehicle restraint systems (refer to dwg RD13.2) ","metre (m)"]
["C3.3.5.2","Asphalt berms placed at existing vehicle restraint systems  (refer to dwg RD13.2) ","metre (m)"]
["C3.3.5.4","Bond coat (30% stable grade emulsion)","square metre (m2)"]
["C3.3.10","Sealed joints in concrete and stone pitched linings of open drains "]
["C3.3.10.1","Silicone sealant (up to 10mm wide, including a closed cell polyethylene backing rope; Silicone sealant to be in accordance with Clause A6.1.5.7c and applied in accordance with the manufacturer's instructions)","metre (m)"]
["C3.3.11","Concrete screed or backfill below chutes (15 MPa concrete)","cubic metre (m3)"]
["C3.3.13","Polymer film sheeting (375 Micron) for concrete-lined open drains","square metre (m2)"]
["C3.3.14","Cutting bituminous surfacing and pavement layers for concrete kerbing, channelling or concrete-lined drains","metre (m)"]
["C3.3.15","Energy dissipaters in outlet structures"]
["C3.3.15.2","Stones set in outlet structures","square metre (m2)"]
["PSC3.3.16","Demolition and removal of existing kerbs and/or channel","cubic metre (m3)"]
["PSC3.3.17","Remove existing kerbing, channelling and edging and set aside for reuse"]
["PSC3.3.17(a)","Precast kerb","metre (m)"]
["PSC3.3.17(b)","Precast channel"]
["PSC3.3.17(b)(i)","Single ","metre (m)"]
["PSC3.3.17(b)(ii)","Double","metre (m)"]
["PSC3.3.17(b)(iii)","Triple","metre (m)"]
["PSC3.3.17(c)","Precast kerb and channel","metre (m)"]
["PSC3.3.17(d)","Precast edging","metre (m)"]
["PSC3.3.17(e)","Extra-over for item PSC3.3.17(a)-(d) for removing granite kerbing, channelling and edging","metre (m)"]
["PSC3.3.18","Relay existing concrete kerbing and/or channelling and edging"]
["PSC3.3.18(a)","Precast kerb only","metre (m)"]
["PSC3.3.18(b)","Precast channel only"]
["PSC3.3.18(b)(i)","Single ","metre (m)"]
["PSC3.3.18(b)(ii)","Double","metre (m)"]
["PSC3.3.18(b)(iii)","Triple","metre (m)"]
["PSC3.3.18(c)","Precast kerb and channel","metre (m)"]
["PSC3.3.18(d)","Precast edging - Type E3","metre (m)"]
["PSC3.3.18(e)","Precast edging - Type E1","metre (m)"]
["PSC3.3.18(f)","Extra-over for item PSC3.3.18(a)-(e) for relaying granite kerbing, channelling and edging","metre (m)"]
["PSC3.3.19","Special backfilling of kerbs using:"]
["PSC3.3.19(a)","G5 quality material from commercial sources","cubic metre (m3)"]
["PSC3.3.19(b)","Reclaimed Asphalt from site","cubic metre (m3)"]
["PSC3.3.19(c)","Reclaimed asphalt from depot, including loading and free-haul up to 5km","cubic metre (m3)"]
["PSC3.3.20","New concrete chutes or repair of existing concrete chutes","cubic metre (m3)"]
["CHAPTER 8: REPAIR EXISTING LAYERS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["ITEM","DESCRIPTION","UNIT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["SECTION 8.8: PATCHING AND EDGE BREAK REPAIR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C8.8.1","Saw cutting pavement layers for patching"]
["C8.8.1.1","Asphalt or bituminous surfacing to an average depth"]
["C8.8.1.1(a)","Not exceeding 50mm","metre (m)"]
["C8.8.1.1(b)","Exceeding 50mm but not exceeding 100mm","metre (m)"]
["C8.8.1.1(c)","Exceeding 100mm","metre (m)"]
["C8.8.1.2","Cemented pavement layers to an average depth"]
["C8.8.1.2(a)","Not exceeding 100mm","metre (m)"]
["C8.8.1.2(b)","Exceeding 100mm but not exceeding 200mm","metre (m)"]
["C8.8.1.2(c)","Exceeding 200mm","metre (m)"]
["C8.8.1.3","Granular layers to an average depth"]
["C8.8.1.3(a)","Not exceeding 100mm","metre (m)"]
["C8.8.1.3(b)","Not exceeding 200mm","metre (m)"]
["C8.8.1.3(c)","Exceeding 200mm","metre (m)"]
["C8.8.2","Excavation in existing pavements for patching (non-milling)"]
["C8.8.2.1","Asphalt layers"]
["C8.8.2.1(a)","Not exceeding 10 m² including for edge repairs wider than 250mm","cubic metre (m3)"]
["C8.8.2.1(b)","Exceeding 10 m² but not exceeding 50 m² including for edge repairs wider than 250mm","cubic metre (m3)"]
["C8.8.2.1(c)","Exceeding 50 m² up to 100 m² including for edge repairs wider than 250mm","cubic metre (m3)"]
["C8.8.2.1(d)","Exceeding 100 m²","cubic metre (m3)"]
["C8.8.2.2","Cemented layers"]
["C8.8.2.2(a)","Not exceeding 10 m² including for edge repairs wider than 250mm","cubic metre (m3)"]
["C8.8.2.2(b)","Exceeding 10 m² but not exceeding 50 m² including for edge repairs wider than 250mm ","cubic metre (m3)"]
["C8.8.2.2(c)","Exceeding 50 m² up to 100 m² including for edge repairs wider than 250mm","cubic metre (m3)"]
["C8.8.2.2(d)","Exceeding 100 m²","cubic metre (m3)"]
["C8.8.2.3","Other layers (granular layers)"]
["C8.8.2.3(a)","Not exceeding 10 m² including for edge repairs wider than 250mm","cubic metre (m3)"]
["C8.8.2.3(b)","Exceeding 10 m² but not exceeding 50 m² including for edge repairs wider than 250mm","cubic metre (m3)"]
["C8.8.2.3(c)","Exceeding 50 m² up to 100 m² including for edge repairs wider than 250mm","cubic metre (m3)"]
["C8.8.2.3(d)","Exceeding 100 m²","cubic metre (m3)"]
["C8.8.3","Compacting the floor of excavations for patching (compacted in 150mm layers and to 100% of maximum dry density for sand and 97% of maximum dry density for gravel)","square metre (m2)"]
["PSC8.8.4","Backfilling of excavations for patching with:"]
["PSC8.8.4.3","Asphalt"]
["PSC8.8.4.3(a)","Continuously graded (sand skeletal) using a PG58V-22 (A-E2) binder with a surface area:"]
["PSC8.8.4.3(a)(i)","Not exceeding 10 m² including for edge repairs wider than 250mm","ton (t)"]
["PSC8.8.4.3(a)(ii)","Exceeding 10 m² but not exceeding 50 m² including for edge repairs wider than 250mm","ton (t)"]
["PSC8.8.4.3(a)(iii)","Exceeding 50 m² up to 100 m² including for edge repairs wider than 250mm","ton (t)"]
["PSC8.8.4.3(a)(iv)","Exceeding 100 m²","ton (t)"]
["PSC8.8.4.3(b)","Cold-mix asphalt: certified by Agrèment SA as a minimum of Class 2 type with a surface area:"]
["PSC8.8.4.3(b)(i)","Not exceeding 10 m² including for edge repairs wider than 250mm","ton (t)"]
["PSC8.8.4.3(b)(ii)","Exceeding 10 m² but not exceeding 50 m² including for edge repairs wider than 250mm","ton (t)"]
["PSC8.8.4.3(b)(iii)","Exceeding 50 m² up to 100 m² including for edge repairs wider than 250mm","ton (t)"]
["PSC8.8.4.3(b)(iv)","Exceeding 100 m²","ton (t)"]
["C8.8.4.4","Granular base material (G4) for a patch with a surface area"]
["C8.8.4.4(a)","Not exceeding 10 m² including for edge repairs wider than 250mm","ton (t)"]
["C8.8.4.4(b)","Exceeding 10 m² but not exceeding 50 m² including for edge repairs wider than 250mm","ton (t)"]
["C8.8.4.4(c)","Exceeding 50 m² up to 100 m² including for edge repairs wider than 250mm","ton (t)"]
["C8.8.4.4(d)","Exceeding 100 m²","ton (t)"]
["PSC8.8.7","Spoiling excavated pavement material not required for backfilling","cubic metre (m3)"]
["PSC8.8.8","Application of waterproofing sealant to asphalt patches","litre (ℓ)"]
["CHAPTER 9: ASPHALT LAYERS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["ITEM","DESCRIPTION","UNIT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["SECTION 9.1: ASPHALT LAYERS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C9.1.1","Asphalt mix designs"]
["C9.1.1.2","Sand skeletal mixes:"]
["C9.1.1.2(e)","Level II mix design (Specialist mix specified by the Engineer)","lump sum"]
["C9.1.3","Application of bond coat"]
["C9.1.3.1","Stable–grade 30% net bitumen emulsion (cationic or anionic). Applied with a calibrated distributer ","litre (ℓ)"]
["C9.1.3.4","Polymer modified bitumen emulsion bond coat (0.45l/m²) ","litre (ℓ)"]
["C9.1.3.5","Polymer modified bitumen emulsion tack coat (0.6l/m² to old dry bituminous surfaces) ","litre (ℓ)"]
["C9.1.8","Surfacing of bridge decks"]
["C9.1.8.2","Surfacing  "]
["C9.1.8.2(a)","Surfacing at bridge joint with PG58V-22 (A-E2), 10mm NMPS, level II, sand skeletal mix"]
["C9.1.8.2(a)(i)","25mm minimum thickness","ton (t)"]
["C9.1.8.2(a)(ii)","30mm minimum thickness","ton (t)"]
["C9.1.8.2(a)(iii)","40mm minimum thickness","ton (t)"]
["C9.1.8.2(a)(iv)","50mm minimum thickness","ton (t)"]
["C9.1.8.2(a)(v)","60mm minimum thickness","ton (t)"]
["C9.1.10","Variation rates  "]
["C9.1.10.1","Bitumen "]
["C9.1.10.1(a)","35/50","ton (t)"]
["C9.1.10.1(b)","50/70","ton (t)"]
["C9.1.10.1(c)","70/100","ton (t)"]
["C9.1.10.2","Aggregate   ","ton (t)"]
["C9.1.10.3","Active filler"]
["C9.1.10.3(a)","Cement","ton (t)"]
["C9.1.10.3(b)","Lime","ton (t)"]
["C9.1.12","Asphalt reinforcing - complete (a high strength, open fibreglass grid, suitable for use as an asphalt reinforcing interlayer)","square metre (m2)"]
["CHAPTER 11: ANCILLARY ROAD WORKS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["ITEM","DESCRIPTION","UNIT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["SECTION 11.1: PITCHING, STONEWORK, CAST IN SITU CONCRETE FOR PROTECTION AGAINST EROSION",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.1.2","Stone pitching",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.1.2.1","Plain stone pitching",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.1.2.1(a)","Method 1","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.1.2.1(b)","Method 2","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.1.2.2","Grouted stone pitching with mortar","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.1.2.3","Grouted stone pitching on a concrete bed ","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC11.1.4","Stone masonry walls:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC11.1.4.4","Repair of stone retaining walls with heritage status","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["CHAPTER 11: ANCILLARY ROAD WORKS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["ITEM","DESCRIPTION","UNIT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["SECTION 11.2: NON-STRUCTURAL GABIONS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.2.2","Surface preparation for bedding the gabion boxes and mattresses","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC11.2.3","Gabion boxes and mattresses:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.2.3.1","Galvanized gabion boxes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.2.3.1(a)","1m x 1m x 1m","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.2.3.1(b)","2m x 1m x 1m","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.2.3.1(c)","1.5m x 1m x 1m","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.2.3.1(d)","1m x 1m x 0.5m","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.2.3.2","PVC coated gabion boxes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.2.3.2(a)","1m x 1m x 1m","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.2.3.2(b)","2m x 1m x 1m","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.2.3.2(c)","1.5m x 1m x 1m","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.2.3.2(d)","1m x 1m x 0.5m","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.2.3.3","Galvanized gabion mattresses ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.2.3.3(a)","2m x 1m x 0.3m","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.2.3.3(b)","3m x 1m x 0.3m","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.2.3.3(c)","6m x 2m x 0.17m","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.2.3.4","PVC-coated gabion mattresses",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.2.3.4(a)","2m x 1m x 0.3m","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.2.3.4(b)","3m x 1m x 0.3m","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.2.3.4(c)","6m x 2m x 0.17m","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC11.2.3.5","Repair of existing gabion boxes and mattresses using existing gabion rock","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.2.4","Geotextile (synthetic fibre grade 3 filter fabric)","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["CHAPTER 11: ANCILLARY ROAD WORKS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["ITEM","DESCRIPTION","UNIT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["SECTION 11.4: ROAD RESTRAINT SYSTEMS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.4.1","Erecting of guardrails at 3,81m spacing",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.4.1.1","Complete galvanized system compliant to SANS 1350:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.4.1.1(a)","On timber posts","metre (m)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.4.1.2","Terminal sections for 3,81 guardrails comprising of:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.4.1.2(a)","End wings to SANS 1350","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.4.1.2(b)","Bullnoses to SANS 1350","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.4.1.2(c)","Bridge adapters to SANS 1350 ","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.4.1.2(f)","Bridge adaptors (including extra rails and posts) (S5023-5003)","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.4.5","Additional guardrail posts for 3,81m systems:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.4.5.1","Timber","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.4.6","Reflective plates",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.4.6.1","Steel plates","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.4.7","Removing existing guardrails:","metre (m)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.4.8","Renovating guardrail material: ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.4.8.1","Painting guardrails, end wings and bullnoses","metre (m)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C11.4.14","Nailing of gang nail plates on top of timber guardrail posts","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["CHAPTER 11: ANCILLARY ROAD WORKS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["ITEM","DESCRIPTION","UNIT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["SECTION 11.5: FENCING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC11.5.9","Repairing existing fences ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC11.5.9.1","Repairing existing fences ","provisional sum",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC11.5.9.2","Handling cost, profit and all other charges in respect of item PSC11.5.9.2","percentage (%)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["CHAPTER 11: ANCILLARY ROAD WORKS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["ITEM","DESCRIPTION","UNIT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["SECTION 11.6: ROAD SIGNS ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC11.6.1","Road signboards with painted or coloured semi-matt background. Symbols, lettering and borders in semi- matt black or in Class I retro-reflective material, where the sign board is constructed from:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC11.6.1.7","Regulatory signs, permanent ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC11.6.1.7(a)","600mm diameter ","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC11.6.1.7(b)","900mm diameter","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC11.6.1.7(c)","1200mm diameter","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC11.6.1.9","Warning signs, permanent ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC11.6.1.9(a)","600mm size ","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC11.6.1.9(b)","900mm size ","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC11.6.1.9(c)","1200mm size","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC11.6.1.9(d)","1500mm size","number (No.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC11.6.1.11","Supplementary plates to permanent regulatory or warning signs ","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["CHAPTER 13: STRUCTURES",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["ITEM","DESCRIPTION","UNIT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["SECTION 13.1: FOUNDATIONS ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.1.3","Excavation:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.1.3.1","Excavating soft material situated within the following successive depth ranges:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.1.3.1(a)","0m up to 1,5m","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.1.3.1(b)","> 1,5m and < 3,0m","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.1.3.1(c)","> 3,0m and < 4,5m","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.1.3.2","Extra over subitem C13.1.3.1 for excavation in hard material  irrespective of depth","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.1.3.4","Extra over subitem C13.1.3.1 for excavation by hand","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.1.3.5","Extra over subitem C13.1.3.1 for excavation in restricted areas","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.1.6","Access and drainage:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.1.6.1","Access","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.1.6.2","Drainage","day",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C13.1.7","Backfill to excavations utilising:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C13.1.7.1","Material from excavation","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C13.1.7.2","Imported material","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C13.1.7.3","Soil cement","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C13.1.10","Haul in excess of 1,0 km on excavated material and on material imported for backfill, foundation fill and fill for caissons","cubic metre kilometre (m3.km)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C13.1.14","Foundation fill consisting of:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C13.1.14.1","Rock fill","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C13.1.14.2","Crushed-stone fill","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C13.1.14.3","Compacted granular material","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C13.1.14.4","Mass concrete (Class C12/15-20)","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["C13.1.14.5","Concrete blinding (max 75mm thick, C12/15-20)","cubic metre (m3)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["CHAPTER 13: STRUCTURES",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["ITEM","DESCRIPTION","UNIT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["SECTION 13.2: FALSEWORK, FORMWORK AND CONCRETE FINISH",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2","Vertical formwork to provide (class of finish indicated as F1, F2, F3 or board) surface finish to (description of member to which applicable)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.1","Class F1 finish to elements as indicated",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.1(a)","Abutments","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.1(b)","Piers","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.1(c)","Walls","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.1(d)","Parapets including endblocks","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.1(e)","Deck longitudinal members","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.1(f)","Deck transverse members","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.1(g)","Deck slabs","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.1(h)","Foundations","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.1(i)","Sidewalks","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.1(j)","Culvert barrel","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.1(k)","Culvert headwall","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.1(l)","Apron slabs and cut off walls","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.2","Class F2 finish to elements as indicated",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.2(a)","Abutments","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.2(b)","Piers","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.2(c)","Walls","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.2(d)","Parapets including endblocks","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.2(e)","Deck longitudinal members","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.2(f)","Deck transverse members","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.2(g)","Deck slabs","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.2(h)","Foundations","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.2(i)","Sidewalks","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.2(j)","Culvert barrel","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.2(k)","Culvert headwall","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.2(l)","Apron slabs and cut off walls","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.3","Class F3 finish to elements as indicated",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.3(a)","Abutments","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.3(b)","Piers","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.3(c)","Walls","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.3(d)","Parapets including endblocks","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.3(e)","Deck longitudinal members","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.3(f)","Deck transverse members","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.3(g)","Deck slabs","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.3(h)","Foundations","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.3(i)","Sidewalks","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.3(j)","Culvert barrel","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.3(k)","Culvert headwall","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.2.3(l)","Apron slabs and cut off walls","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.3","Horizontal formwork to provide (class of finish Indicated as F1, F2, F3 or board) surface finish to (description of member to which applicable)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.3.1","Class F1 finish to elements as indicated",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.3.1(a)","Abutments","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.3.1(b)","Piers","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.3.1(c)","Walls","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.3.1(d)","Parapets including endblocks","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.3.1(e)","Deck longitudinal members","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.3.1(f)","Deck transverse members","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.3.1(g)","Deck slabs","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.3.1(h)","Foundations","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.3.1(i)","Sidewalks","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.3.1(j)","Culvert barrel","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.3.1(k)","Culvert headwall","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.3.1(l)","Apron slabs and cut off walls","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.3.2","Class F2 finish to elements as indicated",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.3.2(a)","Abutments","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.3.2(b)","Piers","square metre (m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A"]
["PSC13.2.3.2(c)","Walls","square metre (m2)"]
["PSC13.2.3.2(d)","Parapets including endblocks","square metre (m2)"]
["PSC13.2.3.2(e)","Deck longitudinal members","square metre (m2)"]
["PSC13.2.3.2(f)","Deck transverse members","square metre (m2)"]
["PSC13.2.3.2(g)","Deck slabs","square metre (m2)"]
["PSC13.2.3.2(h)","Foundations","square metre (m2)"]
["PSC13.2.3.2(i)","Sidewalks","square metre (m2)"]
["PSC13.2.3.2(j)","Culvert barrel","square metre (m2)"]
["PSC13.2.3.2(k)","Culvert headwall","square metre (m2)"]
["PSC13.2.3.2(l)","Apron slabs and cut off walls","square metre (m2)"]
["PSC13.2.3.3","Class F3 finish to elements as indicated"]
["PSC13.2.3.3(a)","Abutments","square metre (m2)"]
["PSC13.2.3.3(b)","Piers","square metre (m2)"]
["PSC13.2.3.3(c)","Walls","square metre (m2)"]
["PSC13.2.3.3(d)","Parapets including endblocks","square metre (m2)"]
["PSC13.2.3.3(e)","Deck longitudinal members","square metre (m2)"]
["PSC13.2.3.3(f)","Deck transverse members","square metre (m2)"]
["PSC13.2.3.3(g)","Deck slabs","square metre (m2)"]
["PSC13.2.3.3(h)","Foundations","square metre (m2)"]
["PSC13.2.3.3(i)","Sidewalks","square metre (m2)"]
["PSC13.2.3.3(j)","Culvert barrel","square metre (m2)"]
["PSC13.2.3.3(k)","Culvert headwall","square metre (m2)"]
["PSC13.2.3.3(l)","Apron slabs and cut off walls","square metre (m2)"]
["PSC13.2.4","Inclined formwork to provide (class of finish indicated as F1, F2, F3 or board) surface finish to (description of member to which applicable)"]
["PSC13.2.4.1","Class F1 finish to elements as indicated"]
["PSC13.2.4.1(a)","Abutments","square metre (m2)"]
["PSC13.2.4.1(b)","Piers","square metre (m2)"]
["PSC13.2.4.1(c)","Walls","square metre (m2)"]
["PSC13.2.4.1(d)","Parapets including endblocks","square metre (m2)"]
["PSC13.2.4.1(e)","Deck longitudinal members","square metre (m2)"]
["PSC13.2.4.1(f)","Deck transverse members","square metre (m2)"]
["PSC13.2.4.1(g)","Deck slabs","square metre (m2)"]
["PSC13.2.4.1(h)","Foundations","square metre (m2)"]
["PSC13.2.4.1(i)","Sidewalks","square metre (m2)"]
["PSC13.2.4.1(j)","Culvert barrel","square metre (m2)"]
["PSC13.2.4.1(k)","Culvert headwall","square metre (m2)"]
["PSC13.2.4.1(l)","Apron slabs and cut off walls","square metre (m2)"]
["PSC13.2.4.2","Class F2 finish to elements as indicated"]
["PSC13.2.4.2(a)","Abutments","square metre (m2)"]
["PSC13.2.4.2(b)","Piers","square metre (m2)"]
["PSC13.2.4.2(c)","Walls","square metre (m2)"]
["PSC13.2.4.2(d)","Parapets including endblocks","square metre (m2)"]
["PSC13.2.4.2(e)","Deck longitudinal members","square metre (m2)"]
["PSC13.2.4.2(f)","Deck transverse members","square metre (m2)"]
["PSC13.2.4.2(g)","Deck slabs","square metre (m2)"]
["PSC13.2.4.2(h)","Foundations","square metre (m2)"]
["PSC13.2.4.2(i)","Sidewalks","square metre (m2)"]
["PSC13.2.4.2(j)","Culvert barrel","square metre (m2)"]
["PSC13.2.4.2(k)","Culvert headwall","square metre (m2)"]
["PSC13.2.4.2(l)","Apron slabs and cut off walls","square metre (m2)"]
["PSC13.2.4.3","Class F3 finish to elements as indicated"]
["PSC13.2.4.3(a)","Abutments","square metre (m2)"]
["PSC13.2.4.3(b)","Piers","square metre (m2)"]
["PSC13.2.4.3(c)","Walls","square metre (m2)"]
["PSC13.2.4.3(d)","Parapets including endblocks","square metre (m2)"]
["PSC13.2.4.3(e)","Deck longitudinal members","square metre (m2)"]
["PSC13.2.4.3(f)","Deck transverse members","square metre (m2)"]
["PSC13.2.4.3(g)","Deck slabs","square metre (m2)"]
["PSC13.2.4.3(h)","Foundations","square metre (m2)"]
["PSC13.2.4.3(i)","Sidewalks","square metre (m2)"]
["PSC13.2.4.3(j)","Culvert barrel","square metre (m2)"]
["PSC13.2.4.3(k)","Culvert headwall","square metre (m2)"]
["PSC13.2.4.3(l)","Apron slabs and cut off walls","square metre (m2)"]
["C13.2.6","Formwork to form open joints (description of member to which applicable, and location) "]
["C13.2.6.1","Parapets at expansion joints","square metre (m2)"]
["CHAPTER 13: STRUCTURES"]
["ITEM","DESCRIPTION","UNIT"]
["SECTION 13.3: STEEL REINFORCEMENT"]
["C13.3.1","Reinforcement for:"]
["C13.3.1.1","Parapets including endblocks and Precast Balustrade Types A to Q (to drawing S5023-5010)"]
["C13.3.1.1(a)","Mild-steel bars","ton (t)"]
["C13.3.1.1(b)","High-yield-stress-steel bars (deformed Y-bars)","ton (t)"]
["C13.3.1.2","Precast balustrade top rails Types A to Q (to drawing S5023-5007)"]
["C13.3.1.2(a)","Mild-steel bars","ton (t)"]
["C13.3.1.2(b)","High-yield-stress-steel bars (deformed Y-bars)","ton (t)"]
["C13.3.1.3","Abutments"]
["C13.3.1.3(a)","Mild-steel bars","ton (t)"]
["C13.3.1.3(b)","High-yield-stress-steel bars (deformed Y-bars)","ton (t)"]
["C13.3.1.3(c)","Welded Steel Fabric","kilogram (kg)"]
["C13.3.1.4","Piers"]
["C13.3.1.4(a)","Mild-steel bars","ton (t)"]
["C13.3.1.4(b)","High-yield-stress-steel bars (deformed Y-bars)","ton (t)"]
["C13.3.1.4(c)","Welded Steel Fabric","kilogram (kg)"]
["C13.3.1.5","Walls"]
["C13.3.1.5(a)","Mild-steel bars","ton (t)"]
["C13.3.1.5(b)","High-yield-stress-steel bars (deformed Y-bars)","ton (t)"]
["C13.3.1.5(c)","Welded Steel Fabric","kilogram (kg)"]
["C13.3.1.6","Deck"]
["C13.3.1.6(a)","Mild-steel bars","ton (t)"]
["C13.3.1.6(b)","High-yield-stress-steel bars (deformed Y-bars)","ton (t)"]
["C13.3.1.6(c)","Welded Steel Fabric","kilogram (kg)"]
["C13.3.1.7","Foundations"]
["C13.3.1.7(a)","Mild-steel bars","ton (t)"]
["C13.3.1.7(b)","High-yield-stress-steel bars (deformed Y-bars)","ton (t)"]
["C13.3.1.7(c)","Welded Steel Fabric","kilogram (kg)"]
["C13.3.1.8","Culvert barrels"]
["C13.3.1.8(a)","Mild-steel bars","ton (t)"]
["C13.3.1.8(b)","High-yield-stress-steel bars (deformed Y-bars)","ton (t)"]
["C13.3.1.8(c)","Welded Steel Fabric","kilogram (kg)"]
["C13.3.1.9","Culvert headwalls"]
["C13.3.1.9(a)","Mild-steel bars","ton (t)"]
["C13.3.1.9(b)","High-yield-stress-steel bars (deformed Y-bars)","ton (t)"]
["C13.3.1.9(c)","Welded Steel Fabric","kilogram (kg)"]
["C13.3.1.10","Apron slabs and cut off walls"]
["C13.3.1.10(a)","Mild-steel bars","ton (t)"]
["C13.3.1.10(b)","High-yield-stress-steel bars (deformed Y-bars)","ton (t)"]
["C13.3.1.10(c)","Welded Steel Fabric","kilogram (kg)"]
["C13.3.4","Extra-over item C13.3.1 (a), (b), etc. for galvanising of reinforcement    ","ton (t)"]
["CHAPTER 13: STRUCTURES"]
["ITEM","DESCRIPTION","UNIT"]
["SECTION 13.4: CONCRETE"]
["C13.4.1","Cast in situ concrete (Class of concrete and use or position in structure stated): "]
["C13.4.1.1","Strength concrete (class C):"]
["C13.4.1.1(a)","C12/15-20"]
["C13.4.1.1(a)(i)","Abutments","cubic metre (m3)"]
["C13.4.1.1(a)(ii)","Piers","cubic metre (m3)"]
["C13.4.1.1(a)(iii)","Walls","cubic metre (m3)"]
["C13.4.1.1(a)(iv)","Parapets","cubic metre (m3)"]
["C13.4.1.1(a)(v)","Deck longitudinal members","cubic metre (m3)"]
["C13.4.1.1(a)(vi)","Deck transverse members","cubic metre (m3)"]
["C13.4.1.1(a)(vii)","Deck slabs","cubic metre (m3)"]
["C13.4.1.1(a)(iiv)","Foundations","cubic metre (m3)"]
["C13.4.1.1(a)(iv)","Sidewalks","cubic metre (m3)"]
["C13.4.1.1(a)(v)","Culvert barrel","cubic metre (m3)"]
["C13.4.1.1(a)(vi)","Culvert headwall","cubic metre (m3)"]
["C13.4.1.1(a)(vii)","Apron slabs and cut off walls","cubic metre (m3)"]
["C13.4.1.1(b)","C25/30-20"]
["C13.4.1.1(b)(i)","Abutments","cubic metre (m3)"]
["C13.4.1.1(b)(ii)","Piers","cubic metre (m3)"]
["C13.4.1.1(b)(iii)","Walls","cubic metre (m3)"]
["C13.4.1.1(b)(iv)","Parapets","cubic metre (m3)"]
["C13.4.1.1(b)(v)","Deck longitudinal members","cubic metre (m3)"]
["C13.4.1.1(b)(vi)","Deck transverse members","cubic metre (m3)"]
["C13.4.1.1(b)(vii)","Deck slabs","cubic metre (m3)"]
["C13.4.1.1(b)(iiv)","Foundations","cubic metre (m3)"]
["C13.4.1.1(b)(iv)","Sidewalks","cubic metre (m3)"]
["C13.4.1.1(b)(v)","Culvert barrel","cubic metre (m3)"]
["C13.4.1.1(b)(vi)","Culvert headwall","cubic metre (m3)"]
["C13.4.1.1(b)(vii)","Apron slabs and cut off walls","cubic metre (m3)"]
["C13.4.1.1(c)","C35/40-20"]
["C13.4.1.1(c)(i)","Abutments","cubic metre (m3)"]
["C13.4.1.1(c)(ii)","Piers","cubic metre (m3)"]
["C13.4.1.1(c)(iii)","Walls","cubic metre (m3)"]
["C13.4.1.1(c)(iv)","Parapets","cubic metre (m3)"]
["C13.4.1.1(c)(v)","Deck longitudinal members","cubic metre (m3)"]
["C13.4.1.1(c)(vi)","Deck transverse members","cubic metre (m3)"]
["C13.4.1.1(c)(vii)","Deck slabs","cubic metre (m3)"]
["C13.4.1.1(c)(iiv)","Foundations","cubic metre (m3)"]
["C13.4.1.1(c)(iv)","Sidewalks","cubic metre (m3)"]
["C13.4.1.1(c)(v)","Culvert barrel","cubic metre (m3)"]
["C13.4.1.1(c)(vi)","Culvert headwall","cubic metre (m3)"]
["C13.4.1.1(c)(vii)","Apron slabs and cut off walls","cubic metre (m3)"]
["C13.4.1.2(c)","Durable concrete (class D):"]
["C13.4.1.2(a)","D25/30-XC4(100)-20"]
["C13.4.1.2(a)(i)","Abutments","cubic metre (m3)"]
["C13.4.1.2(a)(ii)","Piers","cubic metre (m3)"]
["C13.4.1.2(a)(iii)","Walls","cubic metre (m3)"]
["C13.4.1.2(a)(iv)","Parapets","cubic metre (m3)"]
["C13.4.1.2(a)(v)","Deck longitudinal members","cubic metre (m3)"]
["C13.4.1.2(a)(vi)","Deck transverse members","cubic metre (m3)"]
["C13.4.1.2(a)(vii)","Deck slabs","cubic metre (m3)"]
["C13.4.1.2(a)(iiv)","Foundations","cubic metre (m3)"]
["C13.4.1.2(a)(iv)","Sidewalks","cubic metre (m3)"]
["C13.4.1.2(a)(v)","Culvert barrel","cubic metre (m3)"]
["C13.4.1.2(a)(vi)","Culvert headwall","cubic metre (m3)"]
["C13.4.1.2(a)(vii)","Apron slabs and cut off walls","cubic metre (m3)"]
["C13.4.1.2(b)","D35/40-XC4(100)-20"]
["C13.4.1.2(b)(i)","Abutments","cubic metre (m3)"]
["C13.4.1.2(b)(ii)","Piers","cubic metre (m3)"]
["C13.4.1.2(b)(iii)","Walls","cubic metre (m3)"]
["C13.4.1.2(b)(iv)","Parapets","cubic metre (m3)"]
["C13.4.1.2(b)(v)","Deck longitudinal members","cubic metre (m3)"]
["C13.4.1.2(b)(vi)","Deck transverse members","cubic metre (m3)"]
["C13.4.1.2(b)(vii)","Deck slabs","cubic metre (m3)"]
["C13.4.1.2(b)(iiv)","Foundations","cubic metre (m3)"]
["C13.4.1.2(b)(iv)","Sidewalks","cubic metre (m3)"]
["C13.4.1.2(b)(v)","Culvert barrel","cubic metre (m3)"]
["C13.4.1.2(b)(vi)","Culvert headwall","cubic metre (m3)"]
["C13.4.1.2(b)(vii)","Apron slabs and cut off walls","cubic metre (m3)"]
["C13.4.1.2(c)","D25/30-XS1(100)-20"]
["C13.4.1.2(c)(i)","Abutments","cubic metre (m3)"]
["C13.4.1.2(c)(ii)","Piers","cubic metre (m3)"]
["C13.4.1.2(c)(iii)","Walls","cubic metre (m3)"]
["C13.4.1.2(c)(iv)","Parapets","cubic metre (m3)"]
["C13.4.1.2(c)(v)","Deck longitudinal members","cubic metre (m3)"]
["C13.4.1.2(c)(vi)","Deck transverse members","cubic metre (m3)"]
["C13.4.1.2(c)(vii)","Deck slabs","cubic metre (m3)"]
["C13.4.1.2(c)(iiv)","Foundations","cubic metre (m3)"]
["C13.4.1.2(c)(iv)","Sidewalks","cubic metre (m3)"]
["C13.4.1.2(c)(v)","Culvert barrel","cubic metre (m3)"]
["C13.4.1.2(c)(vi)","Culvert headwall","cubic metre (m3)"]
["C13.4.1.2(c)(vii)","Apron slabs and cut off walls","cubic metre (m3)"]
["C13.4.1.2(d)","D35/40-XS1(100)-20"]
["C13.4.1.2(d)(i)","Abutments","cubic metre (m3)"]
["C13.4.1.2(d)(ii)","Piers","cubic metre (m3)"]
["C13.4.1.2(d)(iii)","Walls","cubic metre (m3)"]
["C13.4.1.2(d)(iv)","Parapets","cubic metre (m3)"]
["C13.4.1.2(d)(v)","Deck longitudinal members","cubic metre (m3)"]
["C13.4.1.2(d)(vi)","Deck transverse members","cubic metre (m3)"]
["C13.4.1.2(d)(vii)","Deck slabs","cubic metre (m3)"]
["C13.4.1.2(d)(iiv)","Foundations","cubic metre (m3)"]
["C13.4.1.2(d)(iv)","Sidewalks","cubic metre (m3)"]
["C13.4.1.2(d)(v)","Culvert barrel","cubic metre (m3)"]
["C13.4.1.2(d)(vi)","Culvert headwall","cubic metre (m3)"]
["C13.4.1.2(d)(vii)","Apron slabs and cut off walls","cubic metre (m3)"]
["PSC13.4.5","Curing and surface protection of cast in situ concrete, as and where specifically required:"]
["PSC13.4.5.1","Curing using formwork that is retained in place for full curing period"]
["PSC13.4.5.1(a)","Abutments","square metre (m2)"]
["PSC13.4.5.1(b)","Piers","square metre (m2)"]
["PSC13.4.5.1(c)","Walls","square metre (m2)"]
["PSC13.4.5.1(d)","Parapets","square metre (m2)"]
["PSC13.4.5.1(e)","Deck longitudinal members","square metre (m2)"]
["PSC13.4.5.1(f)","Deck transverse members","square metre (m2)"]
["PSC13.4.5.1(g)","Deck slabs","square metre (m2)"]
["PSC13.4.5.1(h)","Foundations","square metre (m2)"]
["PSC13.4.5.1(i)","Sidewalks","square metre (m2)"]
["PSC13.4.5.1(j)","Culvert barrel","square metre (m2)"]
["PSC13.4.5.1(k)","Culvert headwall","square metre (m2)"]
["PSC13.4.5.1(l)","Apron slabs and cut off walls","square metre (m2)"]
["PSC13.4.5.2","Curing using water ponding or constantly spraying exposed surfaces with water"]
["PSC13.4.5.2(a)","Abutments","square metre (m2)"]
["PSC13.4.5.2(b)","Piers","square metre (m2)"]
["PSC13.4.5.2(c)","Walls","square metre (m2)"]
["PSC13.4.5.2(d)","Parapets","square metre (m2)"]
["PSC13.4.5.2(e)","Deck longitudinal members","square metre (m2)"]
["PSC13.4.5.2(f)","Deck transverse members","square metre (m2)"]
["PSC13.4.5.2(g)","Deck slabs","square metre (m2)"]
["PSC13.4.5.2(h)","Foundations","square metre (m2)"]
["PSC13.4.5.2(i)","Sidewalks","square metre (m2)"]
["PSC13.4.5.2(j)","Culvert barrel","square metre (m2)"]
["PSC13.4.5.2(k)","Culvert headwall","square metre (m2)"]
["PSC13.4.5.2(l)","Apron slabs and cut off walls","square metre (m2)"]
["PSC13.4.5.3","Curing using an approved curing compound"]
["PSC13.4.5.3(a)","Abutments","square metre (m2)"]
["PSC13.4.5.3(b)","Piers","square metre (m2)"]
["PSC13.4.5.3(c)","Walls","square metre (m2)"]
["PSC13.4.5.3(d)","Parapets","square metre (m2)"]
["PSC13.4.5.3(e)","Deck longitudinal members","square metre (m2)"]
["PSC13.4.5.3(f)","Deck transverse members","square metre (m2)"]
["PSC13.4.5.3(g)","Deck slabs","square metre (m2)"]
["PSC13.4.5.3(h)","Foundations","square metre (m2)"]
["PSC13.4.5.3(i)","Sidewalks","square metre (m2)"]
["PSC13.4.5.3(j)","Culvert barrel","square metre (m2)"]
["PSC13.4.5.3(k)","Culvert headwall","square metre (m2)"]
["PSC13.4.5.3(l)","Apron slabs and cut off walls","square metre (m2)"]
["PSC13.4.5.4","Curing using plastic sheeting covering, covering with clean sand or absorbant moisture retaining mats"]
["PSC13.4.5.4(a)","Abutments","square metre (m2)"]
["PSC13.4.5.4(b)","Piers","square metre (m2)"]
["PSC13.4.5.4(c)","Walls","square metre (m2)"]
["PSC13.4.5.4(d)","Parapets","square metre (m2)"]
["PSC13.4.5.4(e)","Deck longitudinal members","square metre (m2)"]
["PSC13.4.5.4(f)","Deck transverse members","square metre (m2)"]
["PSC13.4.5.4(g)","Deck slabs","square metre (m2)"]
["PSC13.4.5.4(h)","Foundations","square metre (m2)"]
["PSC13.4.5.4(i)","Sidewalks","square metre (m2)"]
["PSC13.4.5.4(j)","Culvert barrel","square metre (m2)"]
["PSC13.4.5.4(k)","Culvert headwall","square metre (m2)"]
["PSC13.4.5.4(l)","Apron slabs and cut off walls","square metre (m2)"]
["PSC13.4.9","Manufacturing precast concrete members (description of member with reference to drawing)"]
["PSC13.4.9.1","Precast balustrade (drawing S5023-5010),excluding reinforcement"]
["PSC13.4.9.1(a)","Type A precast balustrade (drawing S5023-5010), excluding reinforcement","number (No.)"]
["PSC13.4.9.1(b)","Type B precast balustrade (drawing S5023-5010), excluding reinforcement","number (No.)"]
["PSC13.4.9.1(c)","Type C precast balustrade (drawing S5023-5010), excluding reinforcement","number (No.)"]
["PSC13.4.9.1(d)","Type D precast balustrade (drawing S5023-5010), excluding reinforcement","number (No.)"]
["PSC13.4.9.1(e)","Type E precast balustrade (drawing S5023-5010), excluding reinforcement","number (No.)"]
["PSC13.4.9.1(f)","Type F precast balustrade (drawing S5023-5010), excluding reinforcement","number (No.)"]
["PSC13.4.9.1(g)","Type G precast balustrade (drawing S5023-5010), excluding reinforcement","number (No.)"]
["PSC13.4.9.1(h)","Type H precast balustrade (drawing S5023-5010), excluding reinforcement","number (No.)"]
["PSC13.4.9.1(i)","Type J precast balustrade (drawing S5023-5010), excluding reinforcement","number (No.)"]
["PSC13.4.9.1(j)","Type K precast balustrade (drawing S5023-5010), excluding reinforcement","number (No.)"]
["PSC13.4.9.1(k)","Type L precast balustrade (drawing S5023-5010), excluding reinforcement","number (No.)"]
["PSC13.4.9.1(l)","Type M precast balustrade (drawing S5023-5010), excluding reinforcement","number (No.)"]
["PSC13.4.9.1(m)","Type N precast balustrade (drawing S5023-5010), excluding reinforcement","number (No.)"]
["PSC13.4.9.1(n)","Type P precast balustrade (drawing S5023-5010), excluding reinforcement","number (No.)"]
["PSC13.4.9.1(o)","Type Q precast balustrade (drawing S5023-5010), excluding reinforcement","number (No.)"]
["PSC13.4.9.2","Precast top rails (drawing S5023-5007),excluding reinforcement"]
["PSC13.4.9.2(a)","Type A precast top rails (drawing S5023-5007), excluding reinforcement","number (No.)"]
["PSC13.4.9.2(b)","Type B precast top rails (drawing S5023-5007), excluding reinforcement","number (No.)"]
["PSC13.4.9.2(c)","Type C precast top rails (drawing S5023-5007), excluding reinforcement","number (No.)"]
["PSC13.4.9.2(d)","Type D precast top rails (drawing S5023-5007), excluding reinforcement","number (No.)"]
["PSC13.4.9.2(e)","Type E precast top rails (drawing S5023-5007), excluding reinforcement","number (No.)"]
["PSC13.4.9.2(f)","Type F precast top rails (drawing S5023-5007), excluding reinforcement","number (No.)"]
["PSC13.4.9.2(g)","Type G precast top rails (drawing S5023-5007), excluding reinforcement","number (No.)"]
["PSC13.4.9.2(h)","Type H precast top rails (drawing S5023-5007), excluding reinforcement","number (No.)"]
["PSC13.4.9.2(i)","Type J precast top rails (drawing S5023-5007), excluding reinforcement","number (No.)"]
["PSC13.4.9.2(j)","Type K precast top rails (drawing S5023-5007), excluding reinforcement","number (No.)"]
["PSC13.4.9.2(k)","Type L precast top rails (drawing S5023-5007), excluding reinforcement","number (No.)"]
["PSC13.4.9.2(l)","Type M precast top rails (drawing S5023-5007), excluding reinforcement","number (No.)"]
["PSC13.4.9.2(m)","Type N precast top rails (drawing S5023-5007), excluding reinforcement","number (No.)"]
["PSC13.4.9.2(n)","Type P precast top rails (drawing S5023-5007), excluding reinforcement","number (No.)"]
["PSC13.4.9.2(o)","Type Q precast top rails (drawing S5023-5007), excluding reinforcement","number (No.)"]
["PSC13.4.11","Transporting and erecting precast concrete members including complete installation (description of member with reference to drawing)"]
["PSC13.4.11.1","Precast balustrades (drawing S5023-5010) "]
["PSC13.4.11.1(a)","Type A precast balustrade (drawing S5023-5010) approx 970 kg","number (No.)"]
["PSC13.4.11.1(b)","Type B precast balustrade (drawing S5023-5010) approx 1200 kg","number (No.)"]
["PSC13.4.11.1(c)","Type C precast balustrade (drawing S5023-5010) approx 1360 kg","number (No.)"]
["PSC13.4.11.1(d)","Type D precast balustrade (drawing S5023-5010) approx 1500 kg","number (No.)"]
["PSC13.4.11.1(e)","Type E precast balustrade (drawing S5023-5010) approx 1800 kg","number (No.)"]
["PSC13.4.11.1(f)","Type F precast balustrade (drawing S5023-5010) approx 2000 kg","number (No.)"]
["PSC13.4.11.1(g)","Type G precast balustrade (drawing S5023-5010) approx 2080 kg","number (No.)"]
["PSC13.4.11.1(h)","Type H precast balustrade (drawing S5023-5010) approx 2200 kg","number (No.)"]
["PSC13.4.11.1(i)","Type J precast balustrade (drawing S5023-5010) approx 2340 kg","number (No.)"]
["PSC13.4.11.1(j)","Type K precast balustrade (drawing S5023-5010) approx 2460 kg","number (No.)"]
["PSC13.4.11.1(k)","Type L precast balustrade (drawing S5023-5010) approx 2600 kg","number (No.)"]
["PSC13.4.11.1(l)","Type M precast balustrade (drawing S5023-5010) approx 2800 kg","number (No.)"]
["PSC13.4.11.1(m)","Type N precast balustrade (drawing S5023-5010) approx 2700 kg","number (No.)"]
["PSC13.4.11.1(n)","Type P precast balustrade (drawing S5023-5010) approx 2800 kg","number (No.)"]
["PSC13.4.11.1(o)","Type Q precast balustrade (drawing S5023-5010) approx 3000 kg","number (No.)"]
["PSC13.4.11.2","Precast top rails (drawing S5023-5007)"]
["PSC13.4.11.2(a)","Type A precast top rail (drawing S5023-5007) ","number (No.)"]
["PSC13.4.11.2(b)","Type B precast top rail (drawing S5023-5007)","number (No.)"]
["PSC13.4.11.2(c)","Type C precast top rail (drawing S5023-5007) ","number (No.)"]
["PSC13.4.11.2(d)","Type D precast top rail (drawing S5023-5007) ","number (No.)"]
["PSC13.4.11.2(e)","Type E precast top rail (drawing S5023-5007) ","number (No.)"]
["PSC13.4.11.2(f)","Type F precast top rail (drawing S5023-5007) ","number (No.)"]
["PSC13.4.11.2(g)","Type G precast top rail (drawing S5023-5007) ","number (No.)"]
["PSC13.4.11.2(h)","Type H precast top rail (drawing S5023-5007) ","number (No.)"]
["PSC13.4.11.2(i)","Type J precast top rail (drawing S5023-5007) ","number (No.)"]
["PSC13.4.11.2(j)","Type K precast top rail (drawing S5023-5007) ","number (No.)"]
["PSC13.4.11.2(k)","Type L precast top rail (drawing S5023-5007) ","number (No.)"]
["PSC13.4.11.2(l)","Type M precast top rail (drawing S5023-5007) ","number (No.)"]
["PSC13.4.11.2(m)","Type N precast top rail (drawing S5023-5007) ","number (No.)"]
["PSC13.4.11.2(n)","Type P precast top rail (drawing S5023-5007) ","number (No.)"]
["PSC13.4.11.2(o)","Type Q precast top rail (drawing S5023-5007) ","number (No.)"]
["CHAPTER 13: STRUCTURES"]
["ITEM","DESCRIPTION","UNIT"]
["SECTION 13.6: BEARINGS"]
["PSC13.6.1","Bearings:"]
["PSC13.6.1.1","Bearings (description of each type and class)"]
["PSC13.6.1.1(a)","Elastomeric bearings (200 x 150mm x 48mm)","number (No.)"]
["PSC13.6.1.1(b)","Elastomeric bearings (300 x 150mm x 48mm)","number (No.)"]
["PSC13.6.1.1(c) ","Elastomeric bearings (300 x 200mm x 61mm)","number (No.)"]
["PSC13.6.1.1(d)","Elastomeric bearings (300 x 250mm x 61mm)","number (No.)"]
["PSC13.6.1.1(e)","Elastomeric bearings (400 x 300mm x 61mm)","number (No.)"]
["PSC13.6.1.1(f) ","Elastomeric bearings (400 x 500mm x 77mm)","number (No.)"]
["PSC13.6.1.1(g)","Elastomeric bearings (600 x 450mm x 72mm)","number (No.)"]
["CHAPTER 13: STRUCTURES"]
["ITEM","DESCRIPTION","UNIT"]
["SECTION 13.7: JOINTS"]
["C13.7.1","Expansion joints:"]
["C13.7.1.1","Description of joint"]
["C13.7.1.1(a)","Preformed elastomeric compression seal joint"]
["C13.7.1.1(a)(i)","Up to 20mm width","metre (m)"]
["C13.7.1.1(a)(ii)","20 - 40mm width","metre (m)"]
["C13.7.1.1(a)(i)","40 - 60mm width","metre (m)"]
["C13.7.1.1(a)(ii)","60 - 80mm width","metre (m)"]
["C13.7.1.1(b)","Silicone joint seal (approved silicone sealant including backing chord in accordance with Clause A6.1.5.7c and applied in accordance with the manufacturer's instructions)"]
["C13.7.1.1(b)(i)","Up to 20mm width","metre (m)"]
["C13.7.1.1(b)(ii)","20 - 40mm width","metre (m)"]
["C13.7.1.1(b)(i)","40 - 60mm width","metre (m)"]
["C13.7.1.1(b)(ii)","60 - 80mm width","metre (m)"]
["PSC13.7.4","Sealing joints with:"]
["C13.7.4.1","Sealant (approved silicone sealant including backing chord in accordance with Clause A6.1.5.7c)"]
["C13.7.4.1(a)","0 - 10mm width","metre (m)"]
["C13.7.4.1(b)","10 - 20mm width","metre (m)"]
["PSC13.7.4.3","Filter fabric strips (150mm wide, 340g/m², preimpregnated with bituminous emulsion and bonded across butt-joints using a 60% bituminous emulsion)","metre (m)"]
["PSC13.7.5","Supply and installation of Agrément South Africa certified proprietary expansion joints"]
["PSC13.7.5.1","Claw and other modular joints in nosings"]
["PSC13.7.5.1(a)","40mm claw joint","metre (m)"]
["PSC13.7.5.1(b)","80mm claw joint","metre (m)"]
["PSC13.7.5.2","Asphaltic plug type joints (drawings DET2.1, DET2.2, DET2.3)"]
["PSC13.7.5.2(a)","300mm x 50mm","metre (m)"]
["PSC13.7.5.2(b)","400mm x 75mm","metre (m)"]
["PSC13.7.5.2(c) ","500mm x 100mm","metre (m)"]
["PSC13.7.5.2(g)","Extra over for variation in joint depth of asphaltic joints","litre (ℓ)"]
["PSC13.7.11","Reinstating of expansion gaps in concrete elements ","litre (ℓ)"]
["CHAPTER 13: STRUCTURES"]
["ITEM","DESCRIPTION","UNIT"]
["SECTION 13.8: ANCILLARY STRUCTURAL ELEMENTS"]
["C13.8.5","Steel railings (to detail S5023-5002)","metre (m)"]
["PSC13.8.7","Numbers for structures: (refer to drawings)"]
["C13.8.7.3","Numbers formed in concrete (to detail S5023-5006)","number (No.)"]
["PSC13.8.7.5","Numbers inscribed in existing concrete (to detail S5023-5006)","number (No.)"]
["C13.8.8","Cast in situ no-fines concrete (class of concrete indicated)"]
["C13.8.8.1","C12/15-20","cubic metre (m3)"]
["C13.8.8.2","C25/30-20","cubic metre (m3)"]
["C13.8.8.2","C35/40-20","cubic metre (m3)"]
["C13.8.10","Drainage pipes and weep holes:"]
["C13.8.10.1","Drainage pipes:"]
["C13.8.10.1(a)","uPVC 75-150mm in diameter","metre (m)"]
["C13.8.10.1(b)","uPVC 150-250mm in diameter","metre (m)"]
["C13.8.10.2","Weep holes:"]
["C13.8.10.2(a)","uPVC up to 100mm in diameter","metre (m)"]
["C13.8.12","Synthetic-fibre filter fabric (geotextile grade 1) ","square metre (m²)"]
["C13.8.15","Drainage strips (150mm filter elements)","metre (m)"]
["C13.8.16","Perforated drainage pipes: "]
["C13.8.16.1","65mm diameter perforated drainage pipe wrapped in grade 1 geotextile filter fabric","metre (m)"]
["CHAPTER 13: STRUCTURES"]
["ITEM","DESCRIPTION","UNIT"]
["SECTION 13.12: STRUCTURAL STEEL PROTECTIVE TREATMENT OF MAJOR STRUCTURES"]
["PSC13.12.1","Steelwork protective system:"]
["PSC13.12.1.1","System 6 (COTO section PSA13.12.7.15) or similar approved to existing steelwork on bridges","square metre (m2)"]
["PSC13.12.1.2","System 6 (COTO section PSA13.12.7.15) or similar approved to existing steel handrails ","square metre (m2)"]
["CHAPTER 14: REPAIR OF STRUCTURES"]
["ITEM","DESCRIPTION","UNIT"]
["SECTION 14.1: ACCESS FOR BRIDGE REHABILITATION"]
["C14.1.2","Mobile access units"]
["C14.1.2.1","Establishment of mobile access unit on site (to reach a maximum height of 10m)","lump sum"]
["C14.1.2.2","Setting up of mobile access unit at each structure location and removal after completion","number (No.)"]
["C14.1.2.3","Operation of mobile access unit during repair work at each location (relevant elements of structure)","days"]
["C14.1.2.4","Operation of mobile access unit during inspections by the Engineer","hour (h)"]
["C14.1.2.5","De-establishing and removal of mobile access unit from site after completion of work","lump sum"]
["C14.1.4","Attendance by Rail Authority"]
["C14.1.4.1","Prime cost sum to allow for attendance by the relevant rail authority to obtain access near electrified railway lines or other relevant authorities as required at the repair site ","prime cost (PC) sum"]
["C14.1.4.2","Percentage on prime cost sum for charges and profits","percentage (%)"]
["PSC14.1.8","Temporary access scaffolding platform with minimum 5m² working area"]
["PSC14.1.8.1","Establishment of temporary access scaffolding platform on site"]
["PSC14.1.8.1(a)","For access between 0m and 6m in height"]
["PSC14.1.8.1(a)(i)","Deck","lump sum"]
["PSC14.1.8.1(a)(ii)","Pier","lump sum"]
["PSC14.1.8.1(a)(iiv)","Abutment","lump sum"]
["PSC14.1.8.1(a)(iv)","Walls","lump sum"]
["PSC14.1.8.1(a)(v)","Culvert barrel including headwall","lump sum"]
["PSC14.1.8.1(b)","For access between 6m and 10m in height"]
["PSC14.1.8.1(b)(i)","Deck","lump sum"]
["PSC14.1.8.1(b)(ii)","Pier","lump sum"]
["PSC14.1.8.1(b)(iiv)","Abutment","lump sum"]
["PSC14.1.8.1(b)(iv)","Walls","lump sum"]
["PSC14.1.8.1(b)(v)","Culvert barrel including headwall","lump sum"]
["PSC14.1.8.1(c)","For access greater than 10m in height"]
["PSC14.1.8.1(c)(i)","Deck","lump sum"]
["PSC14.1.8.1(c)(ii)","Pier","lump sum"]
["PSC14.1.8.1(c)(iiv)","Abutment","lump sum"]
["PSC14.1.8.1(c)(iv)","Walls","lump sum"]
["PSC14.1.8.1(c)(v)","Culvert barrel including headwall","lump sum"]
["PSC14.1.8.2","Setting up of temporary access scaffolding platform at each structure location and removal after completion"]
["PSC14.1.8.2(a)","For access between 0m and 6m in height"]
["PSC14.1.8.2(a)(i)","Deck","number (No.)"]
["PSC14.1.8.2(a)(ii)","Pier","number (No.)"]
["PSC14.1.8.2(a)(iiv)","Abutment","number (No.)"]
["PSC14.1.8.2(a)(iv)","Walls","number (No.)"]
["PSC14.1.8.2(a)(v)","Culvert barrel including headwall","number (No.)"]
["PSC14.1.8.2(b)","For access between 6m and 10m in height"]
["PSC14.1.8.2(b)(i)","Deck","number (No.)"]
["PSC14.1.8.2(b)(ii)","Pier","number (No.)"]
["PSC14.1.8.2(b)(iiv)","Abutment","number (No.)"]
["PSC14.1.8.2(b)(iv)","Walls","number (No.)"]
["PSC14.1.8.2(b)(v)","Culvert barrel including headwall","number (No.)"]
["PSC14.1.8.2(c)","For access greater than 10m in height"]
["PSC14.1.8.2(c)(i)","Deck","number (No.)"]
["PSC14.1.8.2(c)(ii)","Pier","number (No.)"]
["PSC14.1.8.2(c)(iiv)","Abutment","number (No.)"]
["PSC14.1.8.2(c)(iv)","Walls","number (No.)"]
["PSC14.1.8.2(c)(v)","Culvert barrel including headwall","number (No.)"]
["PSC14.1.8.3","Operation and maintenance of the temporary access scaffolding platform at each structure location "]
["PSC14.1.8.3(a)","For access between 0m and 6m in height"]
["PSC14.1.8.3(a)(i)","Deck","days"]
["PSC14.1.8.3(a)(ii)","Pier","days"]
["PSC14.1.8.3(a)(iiv)","Abutment","days"]
["PSC14.1.8.3(a)(iv)","Walls","days"]
["PSC14.1.8.3(a)(v)","Culvert barrel including headwall","days"]
["PSC14.1.8.3(b)","For access between 6m and 10m in height"]
["PSC14.1.8.3(b)(i)","Deck","days"]
["PSC14.1.8.3(b)(ii)","Pier","days"]
["PSC14.1.8.3(b)(iiv)","Abutment","days"]
["PSC14.1.8.3(b)(iv)","Walls","days"]
["PSC14.1.8.3(b)(v)","Culvert barrel including headwall","days"]
["PSC14.1.8.3(c)","For access greater than 10m in height"]
["PSC14.1.8.3(c)(i)","Deck","days"]
["PSC14.1.8.3(c)(ii)","Pier","days"]
["PSC14.1.8.3(c)(iiv)","Abutment","days"]
["PSC14.1.8.3(c)(iv)","Walls","days"]
["PSC14.1.8.3(c)(v)","Culvert barrel including headwall","days"]
["PSC14.1.8.4","De-establishing and removal of access scaffolding platform from site after completion of work"]
["PSC14.1.8.4(a)","For access between 0m and 6m in height"]
["PSC14.1.8.4(a)(i)","Deck","lump sum"]
["PSC14.1.8.4(a)(ii)","Pier","lump sum"]
["PSC14.1.8.4(a)(iiv)","Abutment","lump sum"]
["PSC14.1.8.4(a)(iv)","Walls","lump sum"]
["PSC14.1.8.4(a)(v)","Culvert barrel including headwall","lump sum"]
["PSC14.1.8.4(b)","For access between 6m and 10m in height"]
["PSC14.1.8.4(b)(i)","Deck","lump sum"]
["PSC14.1.8.4(b)(ii)","Pier","lump sum"]
["PSC14.1.8.4(b)(iiv)","Abutment","lump sum"]
["PSC14.1.8.4(b)(iv)","Walls","lump sum"]
["PSC14.1.8.4(b)(v)","Culvert barrel including headwall","lump sum"]
["PSC14.1.8.4(c)","For access greater than 10m in height"]
["PSC14.1.8.4(c)(i)","Deck","lump sum"]
["PSC14.1.8.4(c)(ii)","Pier","lump sum"]
["PSC14.1.8.4(c)(iiv)","Abutment","lump sum"]
["PSC14.1.8.4(c)(iv)","Walls","lump sum"]
["PSC14.1.8.4(c)(v)","Culvert barrel including headwall","lump sum"]
["PSC14.1.9","Suspended access platforms to deck "]
["PSC14.1.9.1","Establishment of suspended access platforms on site "]
["PSC14.1.9.1(a)","Deck sides or outside of parapets (5m² platform working area)","lump sum"]
["PSC14.1.9.1(b)","Deck soffit (10m² platform working area)","lump sum"]
["PSC14.1.9.2","Setting up of suspended access platform at each structure location and removal after completion"]
["PSC14.1.9.2(a)","Deck sides or outside of parapets (5m² platform working area)","number (No.)"]
["PSC14.1.9.2(b)","Deck soffit (10m² platform working area)","number (No.)"]
["PSC14.1.9.3","Operation and maintenance of suspended access platform at each structure location"]
["PSC14.1.9.3(a)","Deck sides or outside of parapets (5m² platform working area)","days"]
["PSC14.1.9.3(b)","Deck soffit (10m² platform working area)","days"]
["PSC14.1.9.4","De-establishing and removal of suspended access platform from site after completion of work"]
["PSC14.1.9.4(a)","Deck sides or outside of parapets (5m² platform working area)","lump sum"]
["PSC14.1.9.4(b)","Deck soffit (10m² platform working area)","lump sum"]
["CHAPTER 14: REPAIR OF STRUCTURES"]
["ITEM","DESCRIPTION","UNIT"]
["SECTION 14.2: CORROSION SURVEY METHODS AND TESTING OF NEAR SURFACE CONCRETE PROPERTIES"]
["C14.2.1","Delamination Survey:"]
["C14.2.1.1","Using hammer tapping technique to existing concrete members","square metre (m2)"]
["C14.2.2","Concrete cover survey "]
["C14.2.2.1","Existing concrete members on bridges","square metre (m2)"]
["C14.2.2.2","Existing concrete members on culverts","square metre (m2)"]
["CHAPTER 14: REPAIR OF STRUCTURES"]
["ITEM","DESCRIPTION","UNIT"]
["SECTION 14.3: DEMOLITION AND REMOVAL OF STRUCTURAL CONCRETE AND STEELWORK"]
["C14.3.1","Demolition of concrete members or elements "]
["C14.3.1.2","Partial member or element (location and description)"]
["C14.3.1.2(a)","Abutments","cubic metre (m3)"]
["C14.3.1.2(b)","Piers","cubic metre (m3)"]
["C14.3.1.2(c) ","Walls","cubic metre (m3)"]
["C14.3.1.2(d)","Parapets including enbdlock","cubic metre (m3)"]
["C14.3.1.2(e)","Deck longitudinal members","cubic metre (m3)"]
["C14.3.1.2(f)","Deck transverse members","cubic metre (m3)"]
["C14.3.1.2(g) ","Deck slabs","cubic metre (m3)"]
["C14.3.1.2(h)","Foundations","cubic metre (m3)"]
["C14.3.3","Demolition of structural steel structures, members or elements (location and description)"]
["C14.3.3.2","Partial member or element (location and description)"]
["C14.3.3.2(a)","Steelwork","ton (t)"]
["C14.3.5","Removal of metal sections embedded in concrete (description)"]
["C14.3.5.1","Handrail posts embedded in concrete (pocket size of 120 x 120 x 50mm)","number (No.)"]
["C14.3.5.2","Handrail posts embedded concrete (pocket sizes of 150 x 150 x 50mm)","number (No.)"]
["C14.3.5.3","Grinding exposed stubs of removed handrail posts flush with top of concrete","number (No.)"]
["C14.3.5.4","Cut back tie rods and make good (pocket size 50 x 50 x 50mm)","number (No.)"]
["C14.3.5.5","Cut back or removal of embedded reinforcement and make good (pocket size of 50 x 50 x 50mm)","number (No.)"]
["CHAPTER 14: REPAIR OF STRUCTURES"]
["ITEM","DESCRIPTION","UNIT"]
["SECTION 14.4: SURFACE AND STRUCTURAL REPAIR OF CONCRETE MEMBERS"]
["PSC14.4.3","Proprietary cementitious repair system in accordance with Table A14.4.5-1"]
["PSC14.4.3.1","Class R4 cement-based, shrinkage compensated, low permeablility repair mortar that is suitable for Principle 3, Method 3.1 of EN1504 for hand applied mortar to positions as indicated:"]
["PSC14.4.3.1(a)","Concrete handrails posts and top rails","litre (ℓ)"]
["PSC14.4.3.1(b)","Conrete at joint turnups on parapets","litre (ℓ)"]
["PSC14.4.3.1(c)","Honeycombed concrete on abutments","litre (ℓ)"]
["PSC14.4.3.1(d)","Honeycombed concrete on piers","litre (ℓ)"]
["PSC14.4.3.1(e)","Honeycombed concrete on walls","litre (ℓ)"]
["PSC14.4.3.1(f)","Honeycombed concrete on parapets","litre (ℓ)"]
["PSC14.4.3.1(g)","Honeycombed concrete on deck longitudinal members","litre (ℓ)"]
["PSC14.4.3.1(h)","Honeycombed concrete on deck transverse members","litre (ℓ)"]
["PSC14.4.3.1(i)","Honeycombed concrete on deck slabs","litre (ℓ)"]
["PSC14.4.3.1(j)","Honeycombed concrete on foundations","litre (ℓ)"]
["PSC14.4.3.1(k)","Spalled concrete on abutments","litre (ℓ)"]
["PSC14.4.3.1(l)","Spalled concrete on piers","litre (ℓ)"]
["PSC14.4.3.1(m)","Spalled concrete on walls","litre (ℓ)"]
["PSC14.4.3.1(n)","Spalled concrete on parapets","litre (ℓ)"]
["PSC14.4.3.1(o)","Spalled concrete on deck longitudinal members","litre (ℓ)"]
["PSC14.4.3.1(p)","Spalled concrete on deck transverse members","litre (ℓ)"]
["PSC14.4.3.1(q)","Spalled concrete on deck slabs","litre (ℓ)"]
["PSC14.4.3.1(r)","Spalled concrete on foundations","litre (ℓ)"]
["PSC14.4.3.2","Class R4, self compacting, shrinkage compensated, microconcrete that is suitable for Principle 3, Method 3.2 of EN 1504-9 for recasting with concrete or mortar to positions as indicated:"]
["PSC14.4.3.2(a)","Abutments","litre (ℓ)"]
["PSC14.4.3.2(b)","Piers","litre (ℓ)"]
["PSC14.4.3.2(c)","Walls","litre (ℓ)"]
["PSC14.4.3.2(d)","Parapets including endblocks","litre (ℓ)"]
["PSC14.4.3.2(e)","Deck longitudinal members","litre (ℓ)"]
["PSC14.4.3.2(f)","Deck transverse members","litre (ℓ)"]
["PSC14.4.3.2(g)","Deck slabs","litre (ℓ)"]
["PSC14.4.3.2(h)","Foundations","litre (ℓ)"]
["PSC14.4.3.2(i)","Sidewalks","litre (ℓ)"]
["PSC14.4.3.2(j)","Culvert barrel","litre (ℓ)"]
["PSC14.4.3.2(k)","Culvert headwall","litre (ℓ)"]
["PSC14.4.3.2(l)","Apron slabs and cut off walls","litre (ℓ)"]
["CHAPTER 14: REPAIR OF STRUCTURES"]
["ITEM","DESCRIPTION","UNIT"]
["SECTION 14.5: ANCHORING OF REINFORCEMENT, GROUTING AND CRACK INJECTION"]
["C14.5.1","Anchoring of reinforcing steel:"]
["C14.5.1.1","Reinforcing (type, bar diameter) into formed holes (hole diameter and depth stated) in (description of member) "]
["C14.5.1.1(a)","Reinforcing (Y10 bars) into formed holes (15mm hole diameter, 150mm hole depth) in existing concrete","number (No.)"]
["C14.5.1.1(b)","Reinforcing (Y12 bars) into formed holes (18mm hole diameter, 180mm hole depth) in existing concrete","number (No.)"]
["C14.5.1.1(c)","Reinforcing (Y16 bars) into formed holes (24mm hole diameter, 240mm hole depth) in existing concrete","number (No.)"]
["C14.5.1.1(d)","Reinforcing (Y20 bars) into formed holes (30mm hole diameter, 300mm hole depth) in existing concrete","number (No.)"]
["C14.5.1.1(e)","Reinforcing (Y25 bars) into formed holes (38mm hole diameter, 375mm hole depth) in existing concrete","number (No.)"]
["C14.5.2","Preparation of contact surfaces for grouting (preparation of 1m² of concrete parapet surface for installation of precast top rail)","number (No.)"]
["C14.5.3","Grouting for"]
["C14.5.3.1","Bedding (grouting underneath precast concrete parapets)","litre (ℓ)"]
["C14.5.3.2","Gap filling (filling pockets or holes)","litre (ℓ)"]
["C14.5.4","Establishment on site for crack injection","lump sum"]
["C14.5.5","Surface preparation and surface sealing for crack injection to (location on structure)"]
["C14.5.5.1","Abutments","metre (m)"]
["C14.5.5.2","Piers","metre (m)"]
["C14.5.5.3","Walls","metre (m)"]
["C14.5.5.4","Parapets","metre (m)"]
["C14.5.5.5","Deck","metre (m)"]
["C14.5.5.6","Culvert barrel","metre (m)"]
["C14.5.5.7","Culvert headwall","metre (m)"]
["C14.5.6","Crack injection adhesive to (location on structure)"]
["C14.5.6.1","Abutments","litre (ℓ)"]
["C14.5.6.2","Piers","litre (ℓ)"]
["C14.5.6.3","Walls","litre (ℓ)"]
["C14.5.6.4","Parapets","litre (ℓ)"]
["C14.5.6.5","Deck","litre (ℓ)"]
["C14.5.6.6","Culvert barrel","litre (ℓ)"]
["C14.5.6.7","Culvert headwall","litre (ℓ)"]
["C14.5.7","Crack filling "]
["C14.5.7.1","Repair system to (location on structure)"]
["C14.5.7.1(a)","Abutments","metre (m)"]
["C14.5.7.1(b)","Piers","metre (m)"]
["C14.5.7.1(c)","Walls","metre (m)"]
["C14.5.7.1(d)","Parapets","metre (m)"]
["C14.5.7.1(e)","Deck","metre (m)"]
["C14.5.7.1(f)","Culvert barrel","metre (m)"]
["C14.5.7.1(g)","Culvert headwall","metre (m)"]
["CHAPTER 14: REPAIR OF STRUCTURES"]
["ITEM","DESCRIPTION","UNIT"]
["SECTION 14.7: PROTECTIVE COATINGS AND TREATMENTS FOR CONCRETE"]
["C14.7.1","Cleaning and preparation of concrete surface"]
["C14.7.1.1","Hand scrubbing with water and detergent (to remove curing compounds or membranes, shutter release compounds, corrosion stains, and water-soluble contaminants without inadvertently damaging the concrete appearance and without producing an exposed aggregate finish)","square metre (m2)"]
["C14.7.1.2","High-pressure water-jetting (to remove curing compounds or membranes, shutter release compounds, corrosion stains, and water-soluble contaminants without inadvertently damaging the concrete appearance and without producing an exposed aggregate finish)","square metre (m2)"]
["PSC14.7.2","Application of protective coatings and treatments in accordance with A14.7.5"]
["PSC14.7.2.1","Hydrophobic impregnants","square metre (m2)"]
["PSC14.7.2.2","Sealers and pore blockers","square metre (m2)"]
["PSC14.7.2.3","Coatings"]
["PSC14.7.2.3a","Two coats of Sikalastic 152 or equivalent to exposed concrete surfaces.","square metre (m2)"]
["PSC14.7.2.3b","Application of protective coatings that includes 1 coat of Primer with 2 coats of Sikagard 550W Elastic or equivalent to all concrete surfaces.","square metre (m2)"]
["PSC14.7.2.4","Renderings","square metre (m2)"]
["PSC14.7.2.5","Corrosion inhibitor"]
["PSC14.7.2.5a","Application of Corrosion inhibitor Sika Ferroguard 903 or equivalent to all concrete repair sections","square metre (m2)"]
["PSC14.7.2.5b","Application of Sika Armatec 110 EC or equivalent to all concrete surface areas exposed for repairs and all exposed reinforced steel","square metre (m2)"]
["C14.7.4","Trial sample panels"]
["C14.7.4.1","Hydrophobic impregnants","square metre (m2)"]
["C14.7.4.2","Sealers and pore blockers","square metre (m2)"]
["C14.7.4.3","Coatings","square metre (m2)"]
["C14.7.4.4","Renderings","square metre (m2)"]
["C14.7.4.5","Corrosion inhibitor","square metre (m2)"]
["CHAPTER 14: REPAIR OF STRUCTURES"]
["ITEM","DESCRIPTION","UNIT"]
["SECTION 14.9: REPAIR AND REPLACEMENT OF ANCILLARY STRUCTURAL ELEMENTS"]
["C14.9.2","Clear bridge drainage system (description of elements)"]
["C14.9.2.1","Scuppers","number (No.)"]
["C14.9.2.2","Weepholes","number (No.)"]
["C14.9.2.3","Drainage pipes","number (No.)"]
["PSC14.9.3","Service and repair of existing joint system"]
["PSC14.9.3.1","Cleaning of existing joint grooves","metre (m)"]
["PSC14.9.3.2","Replacement of existing glands in claw type joints up to 80mm wide","metre (m)"]
["PSC14.9.3.3","Refurbishment of existing steel edging in joint, including removal of surface rust and application of a corrosion protection system 6 (COTO section PSA13.12.7.15) or similar approved","square metre (m2)"]
["PSC14.9.3.4","Complete removal and replacement of existing concrete nosing in 40mm claw type joints","litre (ℓ)"]
["PSC14.9.3.5","Complete removal and replacement of existing concrete nosing in 80mm claw type joints","litre (ℓ)"]
["PSC14.9.3.6","Tightening of nuts and bolts","Number (No.)"]
["PSC14.9.3.7","Complete removal and disposal of existing asphaltic plug joint - up to 500 x 100mm","metre (m)"]
["PSC14.9.3.8","Complete removal and disposal of existing 40mm claw joint","metre (m)"]
["PSC14.9.3.9","Complete removal and disposal of existing 80mm claw joint","metre (m)"]
["PSC14.9.3.10","Complete removal and disposal of compression seal type joints up to 40mm wide","metre (m)"]
["PSC14.9.3.11","Complete removal, disposal and replacement of field poured sealant type joints (silicone sealant with backing cord) of up to 20 x 20mm in size","metre (m)"]
["C14.9.4","Joint terminations as specified on the drawings in:"]
["C14.9.4.1","Barriers and Parapets (claw type joint)","number (No.)"]
["C14.9.4.2","Sidewalks (claw type joint)","number (No.)"]
["C14.9.5","Cover plates (non-metallic) in barriers, parapets and sidewalks as specified on the drawings in:"]
["C14.9.5.1","Barriers and parapets"]
["C14.9.5.1(a)","Cover plate on parapets at joint termination (detail S5023-5009)","number (No.)"]
["C14.9.5.1(b)","Service duct cover on parapets (300 x 150mm)","number (No.)"]
["C14.9.5.2","Sidewalks"]
["C14.9.5.2(a)","Cover plate on sidewalks at joint termination (detail S5023-5009)","number (No.)"]
["C14.9.5.2(b)","Service duct cover on sidewalks (300 x 150mm)","number (No.)"]
["PSC14.9.6","Repair of handrails (repair, realignment, reinstallation, or refixing of existing steel handrails)","metre (m)"]
["PSC14.9.7","Removal and reinstatement of brickwork "]
["PSC14.9.7.1","Removal of brickwork","cubic metre (m3)"]
["PSC14.9.7.2","Reinstating or newly constructed brickwork","cubic metre (m3)"]
["C14.9.8","Drilling of drainage holes into void formers from deck soffit (up to 100mm dia.)","number (No.)"]
["PSC14.9.9","Refurbishment of bearings "]
["PSC14.9.9.1","In-situ bearing refurbishment (including removal of surface rust and application of a paint system - System 6 in COTO section PSA13.12.7.15 or similar approved)","square metre (m2)"]
["PSC14.9.9.2","In-situ repair of bearing plinths","litre (ℓ)"]
["C14.9.10","Replace PVC junctions in deck (type and size described)"]
["C14.9.10.1","110mm","number (No.)"]
["C14.9.10.2","150mm","number (No.)"]
["C14.9.16","Supply new ancillary elements"]
["C14.9.16.1","Extend scuppers below deck soffit"]
["C14.9.16.1(a)","Up to 100mm diameter","metre (m)"]
["C14.9.16.1(b)","Greater than 100mm in diameter","metre (m)"]
["PSC14.9.18","Install new drain pipe to bearing shelf (up to 100mm dia.)","metre (m)"]
["CHAPTER 14: REPAIR OF STRUCTURES"]
["ITEM","DESCRIPTION","UNIT"]
["SECTION 14.10: JACKING OF BRIDGE STRUCTURES"]
["PSC14.10.1","Temporary support and foundations"]
["PSC14.10.1.1","Design, construct and erect temporary supports for the jacking of a bridge deck with a capacity at a support as indicated:"]
["PSC14.10.1.1(a)","50 tonnes","number (No.)"]
["PSC14.10.1.1(b)","100 tonnes","number (No.)"]
["PSC14.10.1.2","Dismantle and remove from site all temporary supports with a capacity at a support as indicated:"]
["PSC14.10.1.2(a)","50 tonnes","number (No.)"]
["PSC14.10.1.2(b)","100 tonnes","number (No.)"]
["PSC14.10.2","Jacking equipment"]
["PSC14.10.2.1","Design, supply and install equipment for the jacking of a bridge deck  with a capacity as indicated:"]
["PSC14.10.2.1(a)","50 tonnes","number (No.)"]
["PSC14.10.2.1(b)","100 tonnes","number (No.)"]
["PSC14.10.2.2","Dismantle and remove all jacking equipment from site with a capacity as indicated:"]
["PSC14.10.2.2(a)","50 tonnes","number (No.)"]
["PSC14.10.2.2(b)","100 tonnes","number (No.)"]
["PSC14.10.3","Vertical jacking of the bridge deck ","tonnes (t)"]
["CHAPTER 14: REPAIR OF STRUCTURES"]
["ITEM","DESCRIPTION","UNIT"]
["SECTION 14.11: REPAIR OF STEEL ELEMENTS"]
["C14.11.2","Replacement of rivets or bolts with HSFG bolts (diameter and class indicated)"]
["C14.11.2.1","Class 4.8 bolts"]
["C14.11.2.1(a)","M12","number (No.)"]
["C14.11.2.1(b)","M16","number (No.)"]
["C14.11.2.1(c) ","M20","number (No.)"]
["C14.11.2.1(d)","M24","number (No.)"]
["C14.11.2.1(e)","M30","number (No.)"]
["C14.11.2.1(f)","M36","number (No.)"]
["C14.11.2.2","Class 8.8 bolts"]
["C14.11.2.2(b)","M16","number (No.)"]
["C14.11.2.2(c) ","M20","number (No.)"]
["C14.11.2.2(d)","M24","number (No.)"]
["C14.11.2.2(e)","M30","number (No.)"]
["C14.11.2.2(f)","M36","number (No.)"]
["C14.11.2.3","Class 10.9 bolts"]
["C14.11.2.3(b)","M16","number (No.)"]
["C14.11.2.3(c) ","M20","number (No.)"]
["C14.11.2.3(d)","M24","number (No.)"]
["C14.11.2.3(e)","M30","number (No.)"]
["C14.11.2.3(f)","M36","number (No.)"]
["PSC14.11.3","Removal of damaged or corroded steel members and replacement with new members"]
["PSC14.11.3.1","Removal of damaged or corroded steel members ","kilogram (kg)"]
["PSC14.11.3.2","New replacement steel members including installation","kilogram (kg)"]
["PSC14.11.4","Removal and replacement of roof sheeting on closed bridge walkways"]
["PSC14.11.4.1","Type and thickness of sheeting as indicated"]
["PSC14.11.4.1(a)","Steel IBR roof sheeting (galvanised and painted)"]
["PSC14.11.4.1(a)(i)","0.40mm thick","square metre (m2)"]
["PSC14.11.4.1(a)(ii)","0.48mm thick","square metre (m2)"]
["PSC14.11.4.1(a)(iii)","0.50mm thick","square metre (m2)"]
["PSC14.11.4.1(a)(iv)","0.55mm thick","square metre (m2)"]
["PSC14.11.4.1(a)(v)","0.58mm thick","square metre (m2)"]
["PSC14.11.4.1(a)(vi)","0.80mm thick","square metre (m2)"]
["PSC14.11.4.1(b)","Steel corrugated roof sheeting (galvanised and painted)"]
["PSC14.11.4.1(b)(i)","0.40mm thick","square metre (m2)"]
["PSC14.11.4.1(b)(ii)","0.48mm thick","square metre (m2)"]
["PSC14.11.4.1(b)(iii)","0.50mm thick","square metre (m2)"]
["PSC14.11.4.1(b)(iv)","0.55mm thick","square metre (m2)"]
["PSC14.11.4.1(b)(v)","0.58mm thick","square metre (m2)"]
["PSC14.11.4.1(b)(vi)","0.80mm thick","square metre (m2)"]
["PSC14.11.4.2","Provision for other types of sheeting","provisional sum"]
["PSC14.11.4.3","Handling cost, profit and all other charges in respect of item PSC14.11.4.2","percentage (%)"]
["PSC14.11.5","Re-torquing of bolts on structural steel"]
["PSC14.11.5.1","Bolts up to and including 8mm in diameter","number (No.)"]
["PSC14.11.5.2","Bolts from 12mm to 20mm in diameter","number (No.)"]
["PSC14.11.5.3","Bolts from 20mm to 36mm in diameter","number (No.)"]
["PSC14.11.6","Welding"]
["PSC14.11.6.1","6mm fillet weld","metre (m)"]
["CHAPTER 20: QAULITY ASSURANCE"]
["ITEM","DESCRIPTION","UNIT"]
["SECTION 20.1: TESTING MATERIALS AND JUDGEMENT OF WORKMANSHIP"]
["PSC20.1.6","Provision for commercial laboratory testing"]
["PSC20.1.6(a)","Actual cost of testing","Prov sum"]
["PSC20.1.6(b)","Contractor's charges in respect of subitem C20.1.6(a) above","%"]