{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":82,"n_cols":3,"rows_kept":82}
["Material number","Line No.","Purchase Order Long Text"]
["068013429","      1","PLATE; TYPE: DISHED END, APPLICATION: XMR-20 WAGON, SIDE SAMPLING, MATERIAL: STEEL ASTM A516 GRADE 7"]
["068013429","      2","MM; DRAWING NO: PEW657B0103, LA; SPECIFICATION: PD_PEW_NAT_LET_012, LA; WITH 2 HOLES OF DIA 36 MM.."]
["068013429","      3","TO DRAWING; \n1.PECIAL FEATURES:VACUUM TREATMENT;\n2. CHARPY V-NOTCH IMPACT TEST. (CVN @ -46 DEGREES C"]
["068013429","      4","ION TO BE DONE IN ACCORDANCE WITH SPECIFICATION EN10160: S2E2.\n4. PLATES MUST HAVE A ZERO NEGATIVE T"]
["068013429","      5","NGS / HEAT NUMBER / MATERIAL GRADE TO BE STAMPED USING LOW STRESS DIES.\n6. THE MANUFACTURING PROCESS"]
["068013429","      6","OMOGENEOUS AND CLEAN STEEL. IN ORDER TO MINIMIZE THE NUMBER OF ELONGATED INCLUSIONS, AN INCLUSION SH"]
["068013429","      7","CALCIUM TREATMENT MAY BE USED.\n7. PLATES MUST BE FREE FROM ANY CAVITIES SUCH AS (SCALES, RUST, CRACK"]
["068013429","      8"," CONTENT OF ASTM A516 GRADE 70 TO CONFORM TO MINIMUM 0,2% AND BELOW ALLOWABLE MAXIMUM 0,25 % LIMIT.\n"]
["068013429","      9","ATE WHICH CONFORMS WITH EN 10204 TYPE 3.1 TO BE SUPPLIED ON DELIVERY.\n10. ALL MATERIAL AND MATERIAL"]
["068013429","     10","STAMPED BY AN APPROVED INSPECTION AUTHORITY (AIA) PRIOR TO MANUFACTURING.( AIA TO TRANSFER ALL PLATE"]
["068013429","     11","CEABILITY PURPOSES SUCH AS CAST NUMBERS, HEAT NUMBERS, ROLL NUMBERS ETC)\n11. THE FOLLOWING DOCUMENTA"]
["068013429","     12",":\n(A) MATERIAL INSPECTION CERTIFICATE WHICH CONFROMS WITH EN 10204 TYPE 3.1.\n(B) APPROVED INSPECTION"]
["068019295","      1","PLATE, METALLIC; TYPE: BARREL CAN OUTER OCTENE AND SAFOL-23 WAGON, THICKNESS: 12 MM, WIDTH: 2.897 M,"]
["068019295","      2","2 M, PLATE MATERIAL: STEEL, MATERIAL GRADE: ASTM A516 GRADE 70; DRAWING NO: PEW046C0016, LA; SPECIFI"]
["068019295","      3"," . ITEMS TO BE LASER CUT COMPLETE TO DRAWING; \n1. INSPECTION TO BE DONE BY A GOVERNMENT APPROVED \nIN"]
["068019295","      4","CREDITED WITH SANAS, \nBEFORE ANY CUTTING OR MANUFACTURING OF MATERIAL. \n2.  A DATA PACK TO BE SUPPLI"]
["068019295","      5","LITY AND AIA FOR APPROVAL BEFORE MANUFACTURING CAN\nTAKE PLACE. CONTACT PERSON- TRANSNET QUALITY. \n3."]
["068019295","      6","TION TO BE DISCUSSED WITH THE INSPECTOR, AS THE FINAL PRODUCT SHOULD BE DELIVERED WITH THE INSPECTOR"]
["068019295","      7","LL\nCERTIFICATES INCLUDING THE STAMPED DRAWINGS BY AIA AND THE DATA PACK.\n4. ALL COSTS TO BE INCLUDED"]
["068019298","      1","PLATE, METALLIC;"]
["068019298","      2","TYPE: BARREL CAN CENTRE, OCTENE AND SAFOL-23 WAGON,"]
["068019298","      3","THICKNESS: 12 MM, WIDTH: 2.897 M,"]
["068019298","      4","LENGTH: 8.26 M, DIAMETER: 2.642 M,"]
["068019298","      5","PLATE MATERIAL: STEEL,"]
["068019298","      6","MATERIAL GRADE: ASTM A516 GRADE 70;"]
["068019298","      7","DRAWING NO: PEW046C0020, LA;"]
["068019298","      8","SPECIFICATION: PD_PEW_NAT_LET_012, LA; ."]
["068019298","      9","ITEMS TO BE LASER CUT COMPLETE TO DRAWING;"]
["068019298","     10","1. INSPECTION TO BE DONE BY A GOVERNMENT APPROVED"]
["068019298","     11","INSPECTION AUTHORITY (A.I.A.),"]
["068019298","     12","ACCREDITED WITH SANAS,"]
["068019298","     13","BEFORE ANY CUTTING OR MANUFACTURING OF MATERIAL."]
["068019298","     14","2.  A DATA PACK TO BE SUPPLIED TO TRANSNET ENGINEERING"]
["068019298","     15","Q"]
["068019298","     16","UALITY AND AIA FOR APPROVAL BEFORE MANUFACTURING CAN"]
["068019298","     17","TAKE PLACE. CONTACT PERSON- TRANSNET QUALITY."]
["068019298","     18","3. THE COMPLETE PROCESS OF INSPECTION TO BE DISCUSSED"]
["068019298","     19","WITH THE INSPECTOR, AS THE FINAL PRODUCT SHOULD BE"]
["068019298","     20","DELIVERED WITH THE INSPECTOR'S HARD STAMP ON MATERIAL"]
["068019298","     21","AND ALL CERTIFICATES INCLUDING THE STAMPED DRAWINGS"]
["068019298","     22","BY AIA AND THE DATA PACK."]
["068019298","     23","4. ALL COSTS TO BE INCLUDED IN THE QUOTED PRICE."]
["068019299","      1","PLATE, METALLIC; TYPE: BARREL CAN OUTER OCTENE AND SAFOL-23 WAGON, THICKNESS: 12 MM, WIDTH: 2.897 M,"]
["068019299","      2","2 M, PLATE MATERIAL: STEEL, MATERIAL GRADE: ASTM A516 GRADE 70; DRAWING NO: PEW046C0021, LA; SPECIFI"]
["068019299","      3"," . ITEMS TO BE LASER CUT COMPLETE TO DRAWING; \n1. INSPECTION TO BE DONE BY A GOVERNMENT APPROVED \nIN"]
["068019299","      4","CREDITED WITH SANAS, \nBEFORE ANY CUTTING OR MANUFACTURING OF MATERIAL. \n2.  A DATA PACK TO BE SUPPLI"]
["068019299","      5","LITY AND AIA FOR APPROVAL BEFORE MANUFACTURING CAN\nTAKE PLACE. CONTACT PERSON- TRANSNET QUALITY. \n3."]
["068019299","      6","TION TO BE DISCUSSED WITH THE INSPECTOR, AS THE FINAL PRODUCT SHOULD BE DELIVERED WITH THE INSPECTOR"]
["068019299","      7","LL\nCERTIFICATES INCLUDING THE STAMPED DRAWINGS BY AIA AND THE DATA PACK.\n4. ALL COSTS TO BE INCLUDED"]
["068019350","      1","PLATE, METALLIC; TYPE: CONE OCTENE AND SAFOL-23 WAGON, THICKNESS: 12 MM, WIDTH: 3.271 M, LENGTH: 8.1"]
["068019350","      2","TERIAL GRADE: ASTM A516 GRADE 70; DRAWING NO: PEW046C0022, LA; 1.HEAT TREATMENT: NORMALISED.\n2.SPECI"]
["068019350","      3","\n3.CHARPY V-NOTCH IMPACT TEST. (CVN @ -46 DEGREES CELSIUS).\n4.ULTRASONIC EXAMINATION TO BE DONE IN A"]
["068019350","      4"," 10160: S2E2. \n5.PLATES MUST HAVE A ZERO NEGATIVE TOLERANCE (-0+1).\n6.PLATE MARKINGS / HEAT NUMBER /"]
["068019350","      5","SING #LOW STRESS# DIES.\n7.THE MANUFACTURING PROCESS SHALL BE SELECTED TO PRODUCE HOMOGENEOUS AND CLE"]
["068019350","      6","THE NUMBER OF ELONGATED INCLUSIONS, AN INCLUSION SHAPE CONTROLLED PROCESS SUCH AS CALCIUM TREATMENT"]
["068019350","      7","REE FROM ANY CAVITIES SUCH AS (SCALES, RUST, CRACKS,OIL, ETC,)#\n9.MATERIAL CARBON CONTENT TO CONFORM"]
["068019350","      8","WABLE MAXIMUM 0,25 % LIMIT.\n10.MATERIAL INSPECTION CERTIFICATE WHICH CONFORMS WITH EN 10204 TYPE 3.1"]
["068019350","      9",".ALL MATERIAL AND MATERIAL CERTIFICATE TO BE VERIFIED AND STAMPED BY AN APPROVED INSPECTION AUTHORIT"]
["068019350","     10","( AIA TO TRANSFER ALL IDENTIFICATION NUMBERS FOR TRACEABILITY PURPOSES SUCH AS CAST NUMBERS, HEAT NU"]
["068019350","     11","ESPONSIBILITY TO INFORM TRASNSNET FOR APPROVAL OF FIRST ARTICLE INSPECTION (FAI) BEFORE MANUFACTURIN"]
["068019350","     12"," ON THE PURCHASE ORDER.\n13.THE FOLLOWING DOCUMENTATION TO BE SUPPLIED ON DELIVERY:\n\n(A)QUALITY CONTR"]
["068019350","     13",")MATERIAL INSPECTION CERTIFICATE WHICH CONFROMS WITH EN 10204 TYPE 3.1.\n(C)APPROVED INSPECTION AUTHO"]
["068019350","     14","TERAIL CERTIFCIATES SIGNED BY AIA I.E ( RAW MATERIAL ETC).NB: MATERIAL CERTICATES TO ALSO REFLECT IM"]
["068019350","     15","MATERIAL TEST CERTIFICATES SIGNED BY AIA.\n(F)DIMENSIONAL REPORTS FOR THE END PRODUCT\n(G)SUPPLIER UNI"]
["068019350","     16","ED/MARKED ON THE END PRODUCT AND ALSO TO REFLECT ON PRODUCT DOCUMENTATION SUPPLIED."]
["068019351","      1","PLATE, METALLIC; TYPE: DISHED END OCTENE AND SAFOL-23 WAGON, THICKNESS: 16 MM, WIDTH: 2.582 M, LENGT"]
["068019351","      2","PLATE MATERIAL: STEEL, MATERIAL GRADE: ASTM A516 GRADE 70; DRAWING NO: PEW046C0023, LA; 1.HEAT TREAT"]
["068019351","      3","TURES: VACUUM TREATMENT; \n3.CHARPY V-NOTCH IMPACT TEST. (CVN @ -46 DEGREES CELSIUS).\n4.ULTRASONIC EX"]
["068019351","      4","NCE WITH SPECIFICATION EN 10160: S2E2. \n5.PLATES MUST HAVE A ZERO NEGATIVE TOLERANCE (-0+1).\n6.PLATE"]
["068019351","      5","IAL GRADE TO BE STAMPED USING #LOW STRESS# DIES.\n7.THE MANUFACTURING PROCESS SHALL BE SELECTED TO PR"]
["068019351","      6","EL. IN ORDER TO MINIMIZE THE NUMBER OF ELONGATED INCLUSIONS, AN INCLUSION SHAPE CONTROLLED PROCESS S"]
["068019351","      7"," USED.\n8.PLATES MUST BE FREE FROM ANY CAVITIES SUCH AS (SCALES, RUST, CRACKS,OIL, ETC,)#\n9.MATERIAL"]
["068019351","      8","NIMUM 0,2% AND BELOW ALLOWABLE MAXIMUM 0,25 % LIMIT.\n10.MATERIAL INSPECTION CERTIFICATE WHICH CONFOR"]
["068019351","      9"," SUPPLIED ON DELIVERY.\n11.ALL MATERIAL AND MATERIAL CERTIFICATE TO BE VERIFIED AND STAMPED BY AN APP"]
["068019351","     10",") PRIOR TO MANUFACTURING.( AIA TO TRANSFER ALL IDENTIFICATION NUMBERS FOR TRACEABILITY PURPOSES SUCH"]
["068019351","     11"," ETC)\n12.SUPPLIER HAS A RESPONSIBILITY TO INFORM TRASNSNET FOR APPROVAL OF FIRST ARTICLE INSPECTION"]
["068019351","     12","TOTAL QUANTITY STIPULATED ON THE PURCHASE ORDER.\n13.THE FOLLOWING DOCUMENTATION TO BE SUPPLIED ON DE"]
["068019351","     13","N (QCP) SIGNED BY AIA.\n(B)MATERIAL INSPECTION CERTIFICATE WHICH CONFROMS WITH EN 10204 TYPE 3.1.\n(C)"]
["068019351","     14","AIA) SIGNED REPORT.\n(D)MATERAIL CERTIFCIATES SIGNED BY AIA I.E ( RAW MATERIAL ETC).NB: MATERIAL CERT"]
["068019351","     15","EST REQUIREMENTS.\n(E)ALL MATERIAL TEST CERTIFICATES SIGNED BY AIA.\n(F)DIMENSIONAL REPORTS OF THE END"]
["068019351","     16","IAL NUMBER TO BE REFLECTED/MARKED ON THE END PRODUCT AND ALSO TO REFLECT ON PRODUCT DOCUMENTATION SU"]