{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["BoQ"],"read":"whole","date_system":"1900"}

{"sheet":"BoQ","index":0,"n_rows":40,"n_cols":7,"rows_kept":40,"merged":[[0,1,0,6],[6,2,10,2]]}
[null,"Supply and execution of Rope Access Services as and when needed basis for\nthe Kusile Power Station - Package 20A for the period of 2 years"]
[null,"Detail","SAP Description","QTY","UOM","RATE","Sub - Total"]
[]
[]
[null,"Fixed P&G's"]
[null,"Site Establishment"]
[null,"Office Space and Storage Container","ESTB SITE:MOBILISATION",1,"Sum"]
[null,"Entry Medicals",null,10,"ea"]
[null,"Personal Protective Equipment (PPE)",null,10,"Set Per Person"]
[null,"Safety Harnasses",null,10,"Set Per Person"]
[null,"SHEQ Requirements",null,5,"Set per site"]
[]
[null,"Site De-Establishment"]
[null,"Exit Medicals","PRVD MED SERV:EXIT MEDICAL",10,"per person"]
[null,"Office Space and Storage Container","PAY FEE:FACILITIES FOR CONTRACTOR;DAILY",1,"Sum"]
[]
[null,"Time Related P&G's"]
[null,"Supervisor L3 Rescue Service","HIRE LABR:T10;CS SUPERVISOR;DIPLOMA;5",240,"Month"]
[null,"L1 Technicians Rescue Services","HIRE LABR:TECHNICIAN;TECHNICIAN;DIPLOMA",240,"Month"]
[null,"Transportation Employees (Home - work - Home) Wet Rate","TRNSP PPL:LABOUR;ROAD;AS REQUIRED",24,"Month"]
[null,"Site LDV Wet Rate","MNG TRVL:LDV;DRIVING",8,"Month"]
[]
[null,"Equipment to be supplied (proven cost)"]
[null,"Caribiners","SHACKLE: TYPE: CARIBINDER; DIAMETER: 10 MM; MATERIAL: ALLOY STEEL: HEAT TREATED; LOAD RATING: 25 KN; PIN: 60 MM; INSIDE WIDTH: 50 MM; INSIDE LENGTH: 100 MM; SPECIFICATION: EN362",500,"ea"]
[null,"Double pulley","PULLEY: TYPE: DOUBLE; DIAMETER: 13 MM; MATERIAL: STAINLESS STEEL; GROOVE: TWO; WIDTH: 184 X 108 MM; SPECIFICATION: EN278:07; STRENGTH: 36 KN; UNIT STANDARD: EN 12278:07",25,"ea"]
[null,"Pulley Pro Traction","PULLEY: TYPE: PRO TRACTION; DIAMETER: 11-13 MM; MATERIAL: STAINLESS STEEL; GROOVE: SINGLE; WIDTH: 38 MM; SPECIFICATION: EN 567; STRENGHT: 22KN",25,"ea"]
[null,"Access Pulley","PULLEY: TYPE: ACCESS; DIAMETER: 13 MM; MATERIAL: STAINLESS STEEL; GROOVE: ONE; WIDTH: 88 MM; SPECIFICATION: EN 12278:2007; STRENGHT: 36 KN; SIDE PLATE HEIGHT 130 MM",25,"ea"]
[null,"Access Rig","PULLEY: TYPE: PETZL RESCUE; DIAMETER: 7-13 MM; MATERIAL: ALIMINIUM; GROOVE: SINGLE; WIDTH: 20 MM",40,"ea"]
[null,"Access Rope (Dynamic)","ROPE: MATERIAL: NYLON AND POLYESTER; DIMENSIONS: 11 MM; STRUCTURE: 32 STRAND; MANTLE BRAID; STRENGTH: 2775 KG; TYPE: ACCESS ROPE (DYNAMIC); SPECIFICATION: EN 1891:1998; HIGH DIRT RESISTANCE; BETTER GRIP AND HIGH ABRASION PROTECTION; KERNMATLE DESIGN",1000,"Meter"]
[null,"Access Rope Static","ROPE: MATERIAL: NYLON; LOW STRETCH; DIMENSIONS: 11 MM; STRUCTURE: OUTER PLAIT 16; OUTER BRAID 32; INNER CORE 14; STRENGTH: 2775 KG; TYPE: ACCESS; STATIC; SPECIFICATION: EN 1891:1998",2500,"Meter"]
[null,"Access Sling Round Endless 1.4M","SLING, WIRE ROPE: DIAMETER: 10 MM; ROPE TYPE: ACCESS; ROUND ENDLES; OVERALL LENGTH: 1.4 M; MATERIAL: STEEL GALVANIZED; CAPACITY: 22 KN; SPECIFICATION: EN 566:2017; LEG QUANTITY: 2",100,"ea"]
[null,"Access Sling Wire Rope 1M","SLING, WIRE ROPE: DIAMETER: 10 MM; ROPE TYPE: ACCESS SLING; OVERALL LENGTH: 1 M; CONSTRUCTION: STEEL; MATERIAL: STEEL WIRE; CAPACITY: 1 T; LAY: TWISTED; SPECIFICATION: SO 24300; LEG QUANTITY: 0",250,"ea"]
[null,"APP Cord","CORD: TYPE: APP; LENGTH: 100 M; MATERIAL: POLYESTER BRAID; CONNECTION: CARRIBINDER; WEIGHT: 86 KG; THICKNESS: 8 MM; REC SPECIFICATION: 062513",25,"ea"]
[null,"Rescue rig","RESCUE EQUIPMENT / KIT  CONSISTING OF DESCENDING DEVICE, ROPE MANUFACTURED, TESTED AND MARKED IN ACCORDANCE WITH SANS SPECIFICATIO NS FOR PERSONAL PROTECTIVE EQUIPMENT AGAINST FALLS FROM HEIGHT EQUIPMENTS  SUPPLIED IN A PACKAGE CONTAINING : 1 x ROPE SYSTEM, 20m  LONG, 13mm DIAMETER, MADE FROM POLY-AMIDE MATERIAL TO SANS 50341  1 x DOUBLE OR TRIPLE ACTION KARABINER WITH A CAPTIVE EYE, 25KN, TO SANS 50362 ATTACHED TO THE ROPE WITH A FIGURE 8 OR ALPINE KNOT COVERED WITH A CLEAR PLASTIC HEAT SHRINK SLEEVE 1 x DOUBLE BREAK DECENDING DEVICE TO SANS 50341 WITH A SAFE WORK LOAD OF 150kg  1x WEBBING CUTTER  1 x DOUBLE OR TRIPLE ACTION 25kN KARABINERS ALLUMIN IUM OR STAINLESS STEEL TO SANS 50362 ATTACHED TO THE DESCENDING DEVICE  1 x RED HOLD ALL PROTECTOR BAG  1 x ATTACHMENT STRAP (1.5 m)  TO SANS 50795 (IF REQUIRED)  1 x ETRIER (STEP LOOP) (IF REQUIRED)  1 x FROG CARABINER WITH A TELESCOPIC STICK, 460mm LONG AND EXTEN DABLE TO A LENGTH OF 3.2m IN A HOLD BAG 500mm LONG (IF REQUIRED) * DRAWING D12704 VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER. MATERIAL SPECIFICATION : SANS 5 0341 SECTION 4.1.3 CORROSION SPECIFICATION  : ALL METALLIC COMPONENTS SHALL BE NON CORROSSIVE STANDARD SPECIFICATION : SANS 50351,SANS 50362 AND SANS 50795, ESKOM SPECIFICATION : SCSSCABA5  TEST & CERTIFICATION REQUIREMENTS : CERTIFICATES : TYPE TEST CERTIFICAT ES (AT EVALUATION STAGE).DECLARATION OF CONFORMITY CERTIFICATE (PER PRODUCT SUPPLIED INSTRUCTION FOR USE AND MARKING REQUIREMENTS : DOCUMENT OF THE GENERAL REQUIREMENTS FOR INSTRUCTION FOR USE AND FOR MARKING TO SANS 50365 AND A DOCUMENT ON THE INFORMATION SUPPIED BY THE MANUFACTURER TO SANS 50354, 50355, 50358, 50360, 50361, 50362 AND 50795  IDENTIFICATION : INDELIBLE NUFACTURES TRADEMARK, MODEL NUMBER AND SERIAL NUMBER ON ALL ITEMS \"",5,"ea"]
[null,"Total"]
[null,"Provisional Sums"]
[null,"Life Lines","PAY FEE:PPE REQUIREMENT",1,"Sum",{"v":250000,"d":"R 250,000.00"},{"v":250000,"d":"R 250,000.00"}]
[null,"Accommodation",null,1,"Sum",{"$f":"750*30","v":{"v":22500,"d":"R 22,500.00"}},{"v":2700000,"d":"R 2,700,000.00"}]
[null,"Meals",null,1,"Sum",{"$f":"60*30*2","v":{"v":3600,"d":"R 3,600.00"}},{"v":432000,"d":"R 432,000.00"}]
[null,"Incentive Schemes (no mark-up allowed)","PAY FEE:OTHER (O/T ALLOWABLES)",1,"Sum",{"v":4200000,"d":"R 4,200,000.00"},{"v":4200000,"d":"R 4,200,000.00"}]