{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Tlotlanang"],"not_rendered":{"external_links":1,"defined_names":6},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Tlotlanang","index":0,"n_rows":135,"n_cols":6,"rows_kept":135,"merged":[[0,0,1,5],[2,0,3,5],[5,0,5,5],[6,0,6,5],[134,1,134,4]],"flags":["formulas_cached_only"]}
["TLOTLANANG COMBINED SCHOOL"]
[]
["ELECTRICAL BILL OF QUANTITIES"]
[]
[]
["DEVELOPMENT BANK OF SOUTHERN AFRICA"]
[]
["Item No","Description","Unit","Quantity","Rate","Amount"]
[]
[null,"Lighting and Small Power"]
[]
[1,"400V Kiosk"]
[]
[1.1,"Decommission, Disconnect, Mark all cables, Remove and Store old uncompliate Kiosks","No",1,null,0]
[]
[1.2,"Supply, manufacture, deliver, install 400V and commission new Kiosk complete with all accessories as per the drawings and System specifications.","No",2,null,0]
[]
[2,"SUB-DISTRIBUTION BOARD"]
[]
[null,"Supply, manufacturer,Install and commission 400V SP&L distribution boad complete with all accessories as per the drawing  and System specifications.","No",5,null,0]
[]
[2.1,"Supply, manufacturer,Install and commission 230V SP&L distribution boad complete with all accessories as per the drawing and System specifications.","No",2,null,0]
[]
[3,"LIGHT FITTINGS"]
[]
[3.1,"Suppy, deliver and install the following light fittings complete; inclusive of lamps"]
[]
[3.2,"2X36W 1200mm open channel T5 light fitting ","No",105,null,0]
[]
[3.3,"1X22W IP65 Bulkhead light fitting ","No",50,null,0]
[]
[3.4,"1X22W IP28 Bulkhead light fitting ","No",50,null,0]
[]
[4,"LIGHT SWITCHES"]
[]
[4.1,"Supply, install and connect flush mounted switch unit complete with cover plate, boxes and all accessories"]
[]
[4.2,"Single Lever, 1 Way light switch","No",50,null,0]
[4.3,"Single Lever, 2 Way light switch","No",0]
[]
[4.3,"230V 16A, IP65 Photocell","No",7,null,0]
[]
[5,"CONDUCTORS AND CABLES"]
[]
[5.1,"Supply and install GP PVC insulated copper conductors in required colours drawn into conduit or in trunking"]
[]
["5.1.1","2.5 mm²","m",4000,null,0]
["5.1.2","4 mm² ","m",0]
[]
["5.1.2","6 mm² ","m",2500,null,0]
[]
[5.2,"Supply, deliver and install  PVC, PVC, SWA, PVC  600/1000V cables"]
[]
["5.2.1","70 mm², 4-Core ","m",300,null,0]
[]
["5.2.2","'16 mm², 4-Core","m",500,null,0]
[]
[5.3,"Supply, deliver and install single core antitheft copper coated bare earth conductor"]
[]
["5.3.1","50 mm² single core","m",300,null,0]
[]
["5.3.2","16 mm² single core","m",500,null,0]
{"$rows_empty":20}
[6,"Cable Termination"]
[]
[6.1,"supply, deliver and install termination kit, complete with compression gland, lugs, sleeves and all accessories"]
[]
["6.1.1","70 mm², 4-Core PVC, PVC, SWA, PVC  600/1000V cable","No",8,null,0]
[]
["6.1.2","16 mm², 4-Core PVC, PVC, SWA, PVC  600/1000V cable","No",18,null,0]
[]
["6.1.3","2.5 mm² GP PVC insulated copper conductors","No",120,null,0]
["6.1.5","4 mm² GP PVC insulated copper conductors","No",0]
[]
["6.1.4","6 mm² GP PVC insulated copper conductors","No",120,null,0]
[]
["6.1.5","50 mm² single core antitheft copper coated bare earth conductor","No",8,null,0]
[]
["6.1.6","16 mm² single core antitheft copper coated bare earth conductor","No",18,null,0]
[]
[7,"SWITCHED SOCKET OUTLETS and Isolators"]
[]
[7.1,"Supply, install and connect flush mounted switch socket outlets and isolators as specified including cover plates and all accessories"]
["7.1.1","45A wall mounted isolator ","No",0]
[]
["7.1.1","16 Amp, 3-pin, Standard/Euro combine double switched socket outlet","No",75,null,0]
[]
[8,"Conduit and Conduit Boxes"]
[]
[null,"Supply and install 25mm PVC conduit complete with all accessories including adpters and couplers","No",1200,null,0]
[]
["8.1","'Supply and install 60 mm round, 60 mm deep PVC box for 20 mm conduit fixed in sofit or brickwork or ceiling void","No",140,null,0]
[]
["8.2","Supply and install 100 x 50 x 50 mm galv. box, flush mounted in brickwork","No",60,null,0]
[]
["8.3","'Supply and install 100 x 100 x 50 mm galv. box, flush mounted in brickwork","No",60,null,0]
["  "]
[9,"EXCAVATION AND BACKFILLING"]
[]
[9.1,"Excavate 800mm deep by 500mm wide hand pickable soil","m",800,null,0]
[]
["9.2","Backfilling","m",800,null,0]
[]
[10,"EARTHING AND BONDING"]
[]
["10.1","Perform soil resistivity test","No",1,null,0]
[]
["10.2","Earth and Bond of the complete installation in accordance with the Specifications and SANS Standards.","Sum",1,null,0]
[]
["10.3","Supply, install and test earthing and lightning Protection system","Sum",1,null,0]
[]
[11,"TEST AND COMMISIONING"]
[]
["11.1","Test and Commision the complete installation in accordance with the Specifications and SANS Standards.","Sum",1,null,0]
[]
[null,"TOTAL SUMMARY (Carried to Final Summary Part B: Electrical Works on Page 112 of the MAIN BOQ)",{"$nulls":3},0]