{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["NEW TOOLS SOW"],"not_rendered":{"external_links":1,"defined_names":11},"read":"whole","date_system":"1900"}

{"sheet":"NEW TOOLS SOW","index":0,"n_rows":30,"n_cols":5,"rows_kept":30,"merged":[[1,0,1,4],[2,0,2,1],[29,0,29,3]]}
[]
["SCOPE OF WORK: PROCUREMENT OF NEW TOOLS"]
["Short Format Description",null,null,"Material No.","QTY/Unit"]
[1,"PORTABL EXTRACTION FANS","FAN: TYPE: PORTABLE VENTILATION AND EXTRACTION; DIMENSIONS: WD 1.295 X HT 1.3 M; VOLUME RATING: LOW 21000; HIGH 27600 M3/HR; 220 VOLT; 0.66KW; MOUNTED WITH WHEELS",714628,6]
[2,"VERNIER 300MM STEEL 0.02","CALLIPER, VERNIER: TYPE: DIGI HEIGHT GAUGE; RANGE: 0-300 MM; GRADUATIONS: 0.02 MM; MATERIAL: STEEL; MANUF P/N: 514-102; DIGIMATIC; CARBIDE-TIPPED SCRIBER 07GZA000 FOR 514-102; SCRIBER CLAMP 05GZA033 FOR 514-102",727472,10]
[3,"VACUUM CLEANER:INDUSTRIAL WET AND DRY;80","VACUUM CLEANER: TYPE: INDUSTRIAL WET AND DRY; CAPACITY: 80 L; POWER SOURCE: 3000 W; POTENTIAL: 220-240 V; CURRENT: 16 A",731354,20]
[4,"INSIZE DIGITAL DEPTH GAUGE 300MM","GAUGE, DEPTH: TYPE: 0-300MM DIGITAL DEPTH GAUGE; GRADUATIONS: 0.01 MM; ACCURACY: 0.04 MM; RANGE: 0-300 MM; APPLICATION: MEASURE DEPTH; MATERIAL: STAINLESS STEEL; DISPLAY: DIGITAL",774174,10]
[5,"DETECTOR LEAK INSTR:HELIUM LEAK DETECTOR","DETECTOR, LEAK INSTRUMENT: TYPE: HELIUM LEAK DETECTOR; RANGE: 4 DECADES; REFERENCE NO: P3000XL",784422,4]
[6,"ENDOSCOPE","ENDOSCOPE: TYPE: GENERATOR STATOR AND ROTOR INSPECTION; REFERENCE NO: SL3000LX10-10M",784423,2]
[7,"METER ELECT TEST:INSULATION TESTER","METER, ELECTRICAL TEST: TYPE: INSULATION TESTER; READOUT: LCD SCREEN; RANGE: 1V TO 5KV; SPECIFICATION: IEC 61010-1; REFERENCE NO: 1555FC",784424,2]
[8,"METER ELECT TEST:INSULATION TESTER","METER, ELECTRICAL TEST: TYPE: INSULATION TESTER; READOUT: LCD SCREEN; RANGE: 1V TO 10KV; SPECIFICATION: IEC 61010-1; REFERENCE NO: 1550FC",784425,2]
[9,"METER ELECT TEST:OSCILLOSCOPE;LCD SCREEN","METER, ELECTRICAL TEST: TYPE: OSCILLOSCOPE; READOUT: LCD SCREEN; RANGE: BANDWIDTH 500MHZ; SPECIFICATION: EN61010-1 CATIII 1000V CAT IV 600V; REFERENCE NO: 190-504/S",784426,1]
[10,"METER ELECT TEST:LCD SCREEN","METER, ELECTRICAL TEST: TYPE: ULTRASONIC/DOPPLER TESTER; READOUT: LCD SCREEN; RANGE: FLOW VELOCITY 0.03 TO 82 FT/S; REFERENCE NO: F601",784434,4]
[11,"SAW PWR:CORDLESS MULTI-CUTTER","SAW, POWER: TYPE: CORDLESS MULTI-CUTTER; BLADE SIZE: WD 10 TO 68 MM; CUTTING RANGE: IMMERSION DEPTH 32 TO 100 MM; REFERENCE NO: PRO GOP 185-LI",784468,5]
[12,"WRENCH TRQ:1/2 IN;1500 NM;5:1 RATION","WRENCH, TORQUE: DRIVE SIZE: 1/2 IN; RATING: 1500 NM; GRADUATIONS: 5:1 RATION; LENGTH: 338 MM; REFERENCE NO: KEN5573620K",784469,1]
[13,"WRENCH TRQ:3/4 IN;800 NM;LG 1.235 M","WRENCH, TORQUE: DRIVE SIZE: 3/4 IN; RATING: 800 NM; GRADUATIONS: TORQUE TOLERANCE 3%; LENGTH: 1.235 M; REFERENCE NO: KEN5579757B",784471,1]
[14,"SENSOR:80 DEG C; 1000V","SENSOR: TYPE: CHATTOCK AWM STYLE 21576.25CM; 15M LENGTH; RATING: 80 DEG C; 1000V; REFERENCE NO: EL CID EVOLUTION II",784472,2]
[15,"SENSOR:80 DEG C; 1000V","SENSOR: TYPE: CHATTOCK AWM STYLE 21576.30CM; 15M LENGTH; RATING: 80 DEG C; 1000V; REFERENCE NO: EL CID EVOLUTION II",784473,2]
[16,"SENSOR:80 DEG C; 1000V","SENSOR: TYPE: CHATTOCK AWM STYLE 21576.20CM; 15M LENGTH; RATING: 80 DEG C; 1000V; REFERENCE NO: EL CID EVOLUTION II",784508,2]
[17,"SENSOR:80 DEG C; 1000V","SENSOR: TYPE: CHATTOCK AWM STYLE 21576.10CM; 15M LENGTH; RATING: 80 DEG C; 1000V; REFERENCE NO: EL CID EVOLURION II",784509,2]
[18,"SENSOR:80 DEG C","SENSOR: TYPE: SIGNAL OUTPUT LOOP AWM STYLE 21576; RATING: 80 DEG C; REFERENCE NO: EL CID EVOLUTION II",784510,2]
[19,"SAW PWR:RECIPROCATING;28 MM;1300 W","SAW, POWER: TYPE: RECIPROCATING; BLADE SIZE: 28 MM; STYLE: LOW VIBRATION; RATING: 1300 W; CUTTING RANGE: STROKE LENGTH: 28 MM; REFERENCE NO: PRO GSE 1300 PCE",784515,5]
[20,"SCALE WGH:BENCH DIGITAL;30 KG;1G","SCALE, WEIGH: TYPE: BENCH DIGITAL; CAPACITY: 30 KG; GRADUATIONS: 1G; REFERENCE NO: MICRO CW30",784517,4]
[21,"SENSOR:FIBER OPTIC CABLE","SENSOR: TYPE: FIBER OPTIC CABLE; RATING: 50UM/125UM DUPLEX; REFERENCE NO: MPD 600",784519,1]
[22,"THERMOMETER:INFRARED;0.1 DEG C","THERMOMETER: TYPE: INFRARED; GRADUATIONS: 0.1 DEG C; TEMPERATURE RANGE: -50 TO +1000 DEG C; REFERENCE NO: MT694",784520,4]
[23,"WRENCH CMBTN:SPANNER;38 MM;LG 460 MM","WRENCH, COMBINATION: TYPE: SPANNER; SIZE: 38 MM; LENGTH: 460 MM; STYLE: RING-OPEN END; MATERIAL: CHROME VANADIUM STEEL; REFERENCE NO: EAN 4010886600351",784521,10]
[24,"CABLE ASSY ELECT:500 MM;4","CABLE ASSEMBLY, POWER ELECTRICAL: TYPE: USB INTERFACE TYPE AWN STYLE 2725; OVERALL LENGTH: 500 MM; CONDUCTOR QUANTITY: 4; TERMINATION TYPE: A-TYPE CONNECTOR AND 4 PIN CIRCULAR CONNECTOR; REFERENCE NO: EL CID EVOLUTION II",784528,2]
[25,"CABLE ASSY ELECT:30 M;9","CABLE ASSEMBLY, POWER ELECTRICAL: TYPE: DISTANCE/ENCODER CABLE 1696A AES/EBU 110 OHMS; OVERALL LENGTH: 30 M; CONDUCTOR QUANTITY: 9; TERMINATION TYPE: 9 PIN CIRCULAR CONNECTOR",784529,2]
[26,"STATION:EMERGENCY EYEWASH;FOOT OPERATED","STATION: TYPE: EMERGENCY EYEWASH; FEATURES: FOOT OPERATED; THE EMERGENCY EYEWASH STATION MUST COMPLY WITH THE FOLLOWING SPECIFICATIONS: THE EYEWASH STATION MUST BE A STAND-ALONE AND PEDESTAL-MOUNTED TYPE; FOOT-OPERATED AND SOFT-FLOW NOZZLES; MATERIAL: 304 OR 316 STAINLESS STEEL; HEIGHT 1.1M; COMPLY WITH ANSI/ISEA Z358.1-2014 SPECIFICATION; A FOREIGN MATERIAL EXCLUSION COVER MUST BE FITTED TO THE BOWL THAT CAN BE EASILY REMOVED WHEN THE EYEWASH IS USED; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",785013,1]
["SUB TOTAL",{"$nulls":3},{"$f":"SUM(E4:E29)","v":107}]