{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Pet Scanner Infusion system"],"not_rendered":{"images":1,"defined_names":2},"read":"whole","date_system":"1900"}

{"sheet":"Pet Scanner Infusion system","index":0,"n_rows":39,"n_cols":6,"rows_kept":39,"merged":[[0,0,0,5],[1,0,1,5],[2,0,2,5],[3,0,3,5],[4,0,4,5],[5,0,5,5],[6,0,6,5],[7,0,7,5],[8,0,8,5],[9,0,9,5],[10,0,10,5],[11,0,11,5],[12,0,12,5],[13,0,13,5],[14,0,14,5]]}
["                                                                                                           TENDER SPECIFICATION  ANNEXURE A"]
["GT/GDH/037/2023:THE SUPPLY, DELIVERY, INSTALLATION, COMMISSIONING AND MAINTENANCE OF PET INFUSION SYSTEM FOR STEVE BIKO ACADEMIC HOSPITAL"]
["Note:                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                   "]
["1. Technical Compliance"]
["The bidders must obtain a threshold of 5 points out of a total of 6 points  in respect of specifications(line) with a weight of 1"]
["2. Scoring of the bids"]
["2a. Weight: Each specification will have a weight of 1 or a hash (#), which indicates the level of importance, as follows:   "]
["1 -  A specification with a standard level of importance that must be complied with.,"]
["# -  Indicates a specification with a essential level of importance, where the bid offer will be disqualified, if the specification is not complied with."]
["2b. Score: The Bid Evaluation Committe will assign a score of 0 or1 for each specification, which indicates the level of compliance, as follows:"]
["0 -  The specification does not  comply.     1 -  The specification is fully compliant."]
["2c. Weighted and Total Score: The score will be multiplied by the weight to give the total score for each specification and be added up. "]
["2d. The bidders must comply as follows with the specification: "]
["i. The bidders must comply with all the specifications (line items) with a # weight. "]
["ii. The bidders must obtain a total score of 5 or higher out of 6 points in respect of specifications (line) with a weight of 1."]
["A","B","C","D","E","F"]
["Item no.","Tender Specification","Weight","Comply (Yes/No)","Details of Bid Offer                                            (Provide your answers in this Colum. You are advised to be straight to the point)","Reference to Brochure / Technical Data Sheet (verification)"]
[1,"GENERAL DESCRIPTION: AUTOMATIC DOSE INJECTOR (PET infusion system)"]
["1.1","Pet Infusion system Unit must be mobile with lockable wheels","#"]
["1.2","Pet Infusion system must come with a software.","#"]
["1.3","Must have a prinable dose report","#"]
["1.4","Maximum radioactivity 30 GBq for shielding effectiveness.","#"]
["1.5","Maximun radiopharmaceutical volume 30mls","#"]
["1.6","Dose range 1-30mCi ",1]
["1.7","Dose accuracy ±5% of the measured dose ",1]
["1.8","System radiation profile ≤0.014mSv/hr at 30.5cm from the surface of the cart at maximum activity.",1]
["1.9","Adjustable Flow rate ≤ 1ml/sec","#"]
["1.10","Maximum radiopharmaceutical concentration100mCi/ml",1]
["1.11","Energy range between 25keV-3MeV",1]
["1.12","Must be able to fractionate acitivity doses.","#"]
["1.13","Unit must have clear radiation warning signs","#"]
["1.14","Safety markings must be written in english","#"]
["1.15","Must have an emergency stop button","#"]
["1.16","Must have effective shielding for the user with the surface dose rate less than 1 uSv/h at maximum dose'","#"]
["1.17","Dose calibrator must be incorporated in the unit.","#"]
[]
["2.","Consumables"]
["2.1","Connection tubes (Compatible Patient administration sets), minimum of 20",1]
[null,"TOTAL POINTS",6]