Scope of Work

Randburg, Dover Street Fibre Repairs

1. Installation of 96 Core Blown fibre (UG) cable SM.Fibre to be collected at Sentech Radiokop (STP). Cable length will be determined during the site survey.
2. Removal of the damaged fibre
3. Supply of two dome joints
4. Fibre splicing services.
5. OTDR tests.
6. Fibre fault localization

Location: Main and Dover Street, Randburg