{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["Detailed Pricing Schedule","VMwarePricing Schedule","Prof Services Pricing schedule"],"read":"whole","date_system":"1900"}

{"sheet":"Detailed Pricing Schedule","index":0,"n_rows":725,"n_cols":13,"rows_kept":725,"merged":[[0,1,0,3]]}
[null,"Pricing Summary"]
[null,null,"Total Excluding VAT","Total Including VAT"]
[null,"Dell Pricing",{"$f":"L711","v":{"v":0,"d":"R0.00"}},{"$f":"M711","v":{"v":0,"d":"R0.00"}}]
[null,"Vmware",{"$f":"'VMwarePricing Schedule'!F16","v":{"v":0,"d":"R0.00"}},{"$f":"'VMwarePricing Schedule'!G16","v":{"v":0,"d":"R0.00"}}]
[null,"Professional Service",{"$f":"'Prof Services Pricing schedule'!D8","v":{"v":0,"d":"R0.00"}},{"$f":"'Prof Services Pricing schedule'!E8","v":{"v":0,"d":"R0.00"}}]
[null,"Professional Service Year 2 to 5",{"$f":"'Prof Services Pricing schedule'!D15","v":{"v":0,"d":"R0.00"}},{"$f":"'Prof Services Pricing schedule'!E15","v":{"v":0,"d":"R0.00"}}]
["ExportExcel_SolutionDealId_Label 21925917-"]
[null,"Group Name","Group ID","Product Name","Product Qty","Module Name","Option ID","Option Name","SKUs","Qty","Parent Order Code","Price Excluding VAT","Price Incl VAT"]
[null,"Group 1","4242639.9.1","1. S5248-ON (AZ1) ",2,{"$nulls":6},{"v":0,"d":"R0.00"},{"v":0,"d":"R0.00"}]
[{"$nulls":5},"Operating System","G4S0GLF","OS10 Enterprise, S5248F-ON","[634-BRUN]",1]
[{"$nulls":5},"Base","GPGI6VD","Dell  S5248F-ON Switch, 48x25GbE SFP28, 4x100GbE QSFP28, 2x100GbE QSFP-DD, PSU to IO, 2xPSU","[210-APFB]",1,null,{"v":0,"d":"R0.00"},{"v":0,"d":"R0.00"}]
[{"$nulls":5},"System Documentation","G03L8SJ","User Documentation EMEA 1","[631-ABXS]",1]
[{"$nulls":5},"Power Cords","GABCR4H","Jumper Cord - C13/C14, 2M, 250V, 10A (EU, TW, APCC countries except ANZ)","[450-AFCW]",2]
[{"$nulls":5},"25/40/100G Cables with Embedded Optics","GZ80XFA","Dell Networking Cable, 100GbE, QSFP28 to QSFP28, Passive Copper Direct Attach, 1 Meter","[470-ABOV]",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":5},"Ethernet Optics","G50DQNX","Dell Networking, Transceiver, SFP+, 10GbE, SR, 850nm Wavelength, 300m Reach","[407-BCZR]",8]
[{"$nulls":5},"SFP+ Direct Attach Cables (Twinax, 10GbE)","GF0TWPV","Dell Networking, Cable, SFP28 to SFP28, 25GbE,Passive Copper Twinax Direct Attach Cable,3 Meter","[470-BBCX]",8]
[{"$nulls":5},"SFP+ Direct Attach Cables (Twinax, 10GbE)","GLT0MEV","Dell Networking, Cable, SFP28 to SFP28, 25GbE,Passive Copper Twinax Direct Attach Cable,5 Meter","[470-BBCZ]",10]
[{"$nulls":5},"MultiMode Fiber LC/LC patch cables","GXNWO0U","Dell Networking Cable, OM4 LC/LC  Fiber Cable, (Optics required), 10 Meter","[470-ACMH]",8]
[{"$nulls":5},"Dell Services: OS10 Software Support","GZJ624N","5 Years ProSupport Plus OS10 Enterprise Software Support-Maintenance","[487-14701]",1]
[{"$nulls":5},"Base warranty","G6LK3DT","1Yr Return to Depot - Minimum Warranty","[709-13025], [709-17021], [709-17022], [710-73324]",1]
[{"$nulls":5},"Support Services","GQ578ZL","5Yr ProSupport Plus and 4hr Mission Critical","[528-10337], [865-85507], [865-85508]",1]
[{"$nulls":5},"Dell Services: Deployment Services",947994,"ProDeploy Plus Dell Networking S Series 5XXX Switch","[683-19041], [683-19042], [706-12528]",1]
[null,"Group 2","4242639.9.2","1. S5248-ON (AZ2) ",2]
[{"$nulls":5},"Operating System","G4S0GLF","OS10 Enterprise, S5248F-ON","[634-BRUN]",1]
[{"$nulls":5},"Base","GPGI6VD","Dell  S5248F-ON Switch, 48x25GbE SFP28, 4x100GbE QSFP28, 2x100GbE QSFP-DD, PSU to IO, 2xPSU","[210-APFB]",1]
[{"$nulls":5},"System Documentation","G03L8SJ","User Documentation EMEA 1","[631-ABXS]",1]
[{"$nulls":5},"Power Cords","GABCR4H","Jumper Cord - C13/C14, 2M, 250V, 10A (EU, TW, APCC countries except ANZ)","[450-AFCW]",2]
[{"$nulls":5},"25/40/100G Cables with Embedded Optics","GZ80XFA","Dell Networking Cable, 100GbE, QSFP28 to QSFP28, Passive Copper Direct Attach, 1 Meter","[470-ABOV]",1]
[{"$nulls":5},"Ethernet Optics","G50DQNX","Dell Networking, Transceiver, SFP+, 10GbE, SR, 850nm Wavelength, 300m Reach","[407-BCZR]",8]
[{"$nulls":5},"SFP+ Direct Attach Cables (Twinax, 10GbE)","GF0TWPV","Dell Networking, Cable, SFP28 to SFP28, 25GbE,Passive Copper Twinax Direct Attach Cable,3 Meter","[470-BBCX]",8]
[{"$nulls":5},"SFP+ Direct Attach Cables (Twinax, 10GbE)","GLT0MEV","Dell Networking, Cable, SFP28 to SFP28, 25GbE,Passive Copper Twinax Direct Attach Cable,5 Meter","[470-BBCZ]",10]
[{"$nulls":5},"MultiMode Fiber LC/LC patch cables","GXNWO0U","Dell Networking Cable, OM4 LC/LC  Fiber Cable, (Optics required), 10 Meter","[470-ACMH]",8]
[{"$nulls":5},"Dell Services: OS10 Software Support","GZJ624N","5 Years ProSupport Plus OS10 Enterprise Software Support-Maintenance","[487-14701]",1]
[{"$nulls":5},"Base warranty","G6LK3DT","1Yr Return to Depot - Minimum Warranty","[709-13025], [709-17021], [709-17022], [710-73324]",1]
[{"$nulls":5},"Support Services","GQ578ZL","5Yr ProSupport Plus and 4hr Mission Critical","[528-10337], [865-85507], [865-85508]",1]
[{"$nulls":5},"Dell Services: Deployment Services",947994,"ProDeploy Plus Dell Networking S Series 5XXX Switch","[683-19041], [683-19042], [706-12528]",1]
[null,"Group 3","4242639.9.3","1. S5248-ON (CPT) ",2]
[{"$nulls":5},"Operating System","G4S0GLF","OS10 Enterprise, S5248F-ON","[634-BRUN]",1]
[{"$nulls":5},"Base","GPGI6VD","Dell  S5248F-ON Switch, 48x25GbE SFP28, 4x100GbE QSFP28, 2x100GbE QSFP-DD, PSU to IO, 2xPSU","[210-APFB]",1]
[{"$nulls":5},"System Documentation","G03L8SJ","User Documentation EMEA 1","[631-ABXS]",1]
[{"$nulls":5},"Power Cords","GABCR4H","Jumper Cord - C13/C14, 2M, 250V, 10A (EU, TW, APCC countries except ANZ)","[450-AFCW]",2]
[{"$nulls":5},"25/40/100G Cables with Embedded Optics","GZ80XFA","Dell Networking Cable, 100GbE, QSFP28 to QSFP28, Passive Copper Direct Attach, 1 Meter","[470-ABOV]",1]
[{"$nulls":5},"Ethernet Optics","G50DQNX","Dell Networking, Transceiver, SFP+, 10GbE, SR, 850nm Wavelength, 300m Reach","[407-BCZR]",8]
[{"$nulls":5},"SFP+ Direct Attach Cables (Twinax, 10GbE)","GF0TWPV","Dell Networking, Cable, SFP28 to SFP28, 25GbE,Passive Copper Twinax Direct Attach Cable,3 Meter","[470-BBCX]",8]
[{"$nulls":5},"SFP+ Direct Attach Cables (Twinax, 10GbE)","GLT0MEV","Dell Networking, Cable, SFP28 to SFP28, 25GbE,Passive Copper Twinax Direct Attach Cable,5 Meter","[470-BBCZ]",10]
[{"$nulls":5},"MultiMode Fiber LC/LC patch cables","GXNWO0U","Dell Networking Cable, OM4 LC/LC  Fiber Cable, (Optics required), 10 Meter","[470-ACMH]",12]
[{"$nulls":5},"Dell Services: OS10 Software Support","GZJ624N","5 Years ProSupport Plus OS10 Enterprise Software Support-Maintenance","[487-14701]",1]
[{"$nulls":5},"Base warranty","G6LK3DT","1Yr Return to Depot - Minimum Warranty","[709-13025], [709-17021], [709-17022], [710-73324]",1]
[{"$nulls":5},"Support Services","GQ578ZL","5Yr ProSupport Plus and 4hr Mission Critical","[528-10337], [865-85507], [865-85508]",1]
[{"$nulls":5},"Dell Services: Deployment Services",947994,"ProDeploy Plus Dell Networking S Series 5XXX Switch","[683-19041], [683-19042], [706-12528]",1]
[null,"Group 5","4242639.9.4","PowerEdge R760 Rack Server - [EMEA_R760] ",1]
[{"$nulls":5},"Base","GYF30OW","PowerEdge R760 Server","[210-BDZY]",1]
[{"$nulls":5},"Trusted Platform Module","GGX1VDO","Trusted Platform Module 2.0 V3","[461-AAIG]",1]
[{"$nulls":5},"Chassis Configuration","G0VGW37","2.5\" Chassis with 8 Universal Drive Slots (SAS/SATA/NVME), 2 CPU","[404-BBFB]",1]
[{"$nulls":5},"Processor","G7L5KOQ","Intel® Xeon® Gold 6434 3.7G, 8C/16T, 16GT/s, 23M Cache, Turbo, HT (195W) DDR5-4800","[338-CHSK]",1]
[{"$nulls":5},"Additional Processor","GOA28QZ","Intel® Xeon® Gold 6434 3.7G, 8C/16T, 16GT/s, 23M Cache, Turbo, HT (195W) DDR5-4800","[338-CHSK], [379-BDCO]",1]
[{"$nulls":5},"Processor Thermal Configuration","GALJM2W","Heatsink for 2 CPU configuration (CPU greater than 165W)","[412-ABCP]",1]
[{"$nulls":5},"Memory Configuration Type","GH9QBEI","Performance Optimized","[370-AAIP]",1]
[{"$nulls":5},"Memory DIMM Type and Speed","GGBEML0","4800MT/s RDIMMs","[370-AHCL]",1]
[{"$nulls":5},"Memory Capacity","G1LQYF8","128GB RDIMM, 4800MT/s Quad Rank","[370-AGZM]",12]
[{"$nulls":5},"RAID Configuration","GJ45ICY","C7, Unconfigured RAID for HDDs or SSDs (Mixed Drive Types Allowed)","[780-BCDS]",1]
[{"$nulls":5},"RAID/Internal Storage Controllers","GP6SZU4","PERC H755 with rear load Brackets","[405-AAZB], [750-ADWP]",1]
[{"$nulls":5},"Hard Drives","G3ZJM0K","480GB SSD SATA Read Intensive 6Gbps 512 2.5in Hot-plug AG Drive, 1 DWPD","[400-AXTV]",2]
[{"$nulls":5},"BIOS and Advanced System Configuration Settings","G06TYXW","Power Saving Dell Active Power Controller","[750-AABF]",1]
[{"$nulls":5},"Advanced System Configurations","GSFTG4Y","UEFI BIOS Boot Mode with GPT Partition","[800-BBDM]",1]
[{"$nulls":5},"Fans","G5OU0ID","Standard Fan x6","[750-ADGK]",1]
[{"$nulls":5},"Power Supply","GLJWKU7","Dual, Hot-Plug, FR Power Supply, 1100W MM (100-240Vac) Titanium, Redundant (1+1)","[450-AKKS]",1]
[{"$nulls":5},"Embedded Systems Management","G16CQF5","iDRAC9, Enterprise 16G","[528-CTIC]",1]
[{"$nulls":5},"Power Cords","GDE0CHU","Rack Power Cord 2M (C13/C14 10A)","[450-AADY]",2]
[{"$nulls":5},"PCIe Riser","G1K02HI","Riser Config 2, 2x8 FH Slots (Gen4), 4x8 FH Slots (Gen5), 2x16 LP Slots (Gen4)","[330-BBXY]",1]
[{"$nulls":5},"Motherboard","GSWQBC3","Motherboard supports ONLY CPUs below 250W (cannot upgrade to CPUs 250W and above)","[329-BJLS]",1]
[{"$nulls":5},"OCP 3.0 Network Adapters","GAKY4CT","Broadcom 57504 Quad Port 10/25GbE,SFP28, OCP NIC 3.0","[540-BCRX]",1]
[{"$nulls":5},"Additional Network Cards","GY8XSA9","Broadcom 5720 Dual Port 1GbE Optional LOM","[540-BDKD]",1]
[{"$nulls":5},"Quick Sync","GCLNJM4","No Quick Sync","[350-BBYX]",1]
[{"$nulls":5},"Password","G2T768J","iDRAC,Factory Generated Password","[379-BCSF]",1]
[{"$nulls":5},"Bezel","GWF2PBH","PowerEdge 2U Standard Bezel","[321-BHMY], [325-BEVI]",1]
[{"$nulls":5},"Group Manager","GTVA94K","iDRAC Group Manager, Disabled","[379-BCQY]",1]
[{"$nulls":5},"Boot Optimized Storage Cards","G937ZBP","BOSS-N1 controller card +  with 2 M.2 480GB (RAID 1)","[403-BCRU], [470-AFMF]",1]
[{"$nulls":5},"Operating System","G78MU35","No Operating System","[611-BBBF]",1]
[{"$nulls":5},"OS Media Kits","GKH7AZI","No Media Required","[605-BBFN]",1]
[{"$nulls":5},"Rack Rails","GVERFZ7","ReadyRails Sliding Rails With Cable Management Arm","[770-BDRQ], [770-BEKK]",1]
[{"$nulls":5},"Optics & Cables for Network Cards",null,"Dell Networking, Cable, SFP28 to SFP28, 25GbE, Passive Copper Twinax Direct Attach Cable, 5 Meter","[470-ACEW]",4]
[{"$nulls":5},"System Documentation","GVRYSM7","No Systems Documentation, No OpenManage DVD Kit","[631-AACK]",1]
[{"$nulls":5},"SHIPPING","GK1BRQ7","PowerEdge R760 Shipping EMEA1 (English/French/German/Spanish/Russian/Hebrew)","[340-DKCH]",1]
[{"$nulls":5},"Shipping Material","G6RFPIW","PowerEdge R760 Shipping Material","[340-DJQY]",1]
[{"$nulls":5},"Regulatory","GCN13DP","PowerEdge R760 CE and CCC Marking, No BIS Marking","[343-BBUC]",1]
[{"$nulls":5},"GPU/FPGA/Acceleration Cables","G0PNZWL","No Cables Required, No GPU Blanks","[470-AEYU]",1]
[{"$nulls":5},"Shipping Box Labels - Standard","GDZ0XTY","Order Configuration Shipbox Label (Ship Date, Model, Processor Speed, HDD Size, RAM)","[293-10049]",1]
[{"$nulls":5},"Additional Processor Features","G68EUO7","No HBM","[379-BFFD]",1]
[{"$nulls":5},"Fibre Channel Adapters","G0SWIFX","Emulex LPe35002 Dual Port FC32 Fibre Channel HBA, PCIe Low Profile","[406-BBTM]",1]
[{"$nulls":5},"Dell Services: Hardware Support","G38PX0I","Basic Next Business Day 36 Months, 36 Month(s)","[709-BBIM]",1]
[{"$nulls":5},"Dell Services:Extended Service","GUTGAE9","Prosupport Plus and 4Hr Mission Critical, 60 Month(s)","[865-BBNF], [865-BBNG]",1]
[{"$nulls":5},"Deployment Services",959563,"ProDeploy Plus Dell Server R Series 1U/2U","[683-19204], [683-19205], [706-12474]",1]
[{"$nulls":5},"Anti Theft Device & Asset Tagging","G2K1LTI","Asset Tag - ProSupport (Website, barcode, Onboard MacAddress)","[293-10025]",1]
[null,"Group 5","4242639.9.4","New PowerEdge R660xs Rack Server Domain Controller ",3]
[{"$nulls":5},"Base","GCZ7PSU","PowerEdge R660xs","[210-BFUZ]",1]
[{"$nulls":5},"Trusted Platform Module","GGX1VDO","Trusted Platform Module 2.0 V3","[461-AAIG]",1]
[{"$nulls":5},"Chassis Configuration","GIJKM14","2.5\" Chassis with up to 8 Hard Drives (SAS/SATA), 1 CPU, PERC 11","[470-AFQK]",1]
[{"$nulls":5},"Processor","G9RJCWU","Intel® Xeon® Gold 5416S 2G, 16C/32T, 16GT/s, 30M Cache, Turbo, HT (150W) DDR5-4400","[338-CHSL]",1]
[{"$nulls":5},"Additional Processor","GWSO9LE","No Additional Processor","[374-BBBX]",1]
[{"$nulls":5},"Processor Thermal Configuration","G8RJ6HD","Heatsink for 1 CPU configuration (CPU less than or equal to 150W)","[338-CHQS]",1]
[{"$nulls":5},"Memory Configuration Type","GH9QBEI","Performance Optimized","[370-AAIP]",1]
[{"$nulls":5},"Memory DIMM Type and Speed","GGBEML0","4800MT/s RDIMMs","[370-AHCL]",1]
[{"$nulls":5},"Memory Capacity","GAD7JYE","16GB RDIMM, 4800MT/s Single Rank","[370-AGZO]",6]
[{"$nulls":5},"RAID Configuration","G8510ID","C1, No RAID for HDDs/SSDs (Mixed Drive Types Allowed)","[780-BCDI]",1]
[{"$nulls":5},"RAID Controller","GFMWO9X","Front PERC H355 Front Load","[405-ABCQ], [750-ACFR]",1]
[{"$nulls":5},"Hard Drives","GGMU1EX","1.92TB SSD SATA Read Intensive 6Gbps 512 2.5in Hot-plug AG Drive, 1 DWPD","[400-AXSD]",2]
[{"$nulls":5},"BIOS and Advanced System Configuration Settings","GEARJ9V","Power Saving BIOS Setting","[384-BBBH]",1]
[{"$nulls":5},"Advanced System Configurations","GSFTG4Y","UEFI BIOS Boot Mode with GPT Partition","[800-BBDM]",1]
[{"$nulls":5},"Fans","G64B13H","Standard Fan X5","[384-BDII]",1]
[{"$nulls":5},"Embedded Systems Management","G16CQF5","iDRAC9, Enterprise 16G","[528-CTIC]",1]
[{"$nulls":5},"Power Supply","GTADK34","Dual, Hot-plug, Power Supply Fault Tolerant Redundant (1+1), 800W, Mixed Mode,NAF","[450-AIQX]",1]
[{"$nulls":5},"Power Cords","GDE0CHU","Rack Power Cord 2M (C13/C14 10A)","[450-AADY]",2]
[{"$nulls":5},"PCIe Riser","GFXPN0O","Riser Config 5, Low Profile, 1x16 LP Slots (Gen4) + 1x8 LP Slot (Gen5), 1CPU","[330-BCCF]",1]
[{"$nulls":5},"Motherboard","GF87RXE","PowerEdge R660xs Motherboard with Broadcom 5720 Dual Port 1Gb On-Board LOM","[384-BDKV]",1]
[{"$nulls":5},"Network Daughter Card","G91LG8U","Broadcom 57416 Dual Port 10GbE BASE-T Adapter, OCP NIC 3.0","[540-BCOD]",1]
[{"$nulls":5},"Quick Sync","GT8Y6M9","No Quick Sync","[350-BCEM]",1]
[{"$nulls":5},"Password","G2T768J","iDRAC,Factory Generated Password","[379-BCSF]",1]
[{"$nulls":5},"Group Manager","GTC0D81","iDRAC Group Manager, Enabled","[379-BCQV]",1]
[{"$nulls":5},"Bezel","GO13GT6","Standard Bezel for x8 and x10 chassis","[325-BEUF], [325-BEVH]",1]
[{"$nulls":5},"Operating System","G78MU35","No Operating System","[611-BBBF]",1]
[{"$nulls":5},"OS Media Kits","GKH7AZI","No Media Required","[605-BBFN]",1]
[{"$nulls":5},"Rack Rails","GYVEJ7N","ReadyRails A11 drop-in/stab-in Combo Rails With Cable Management Arm","[770-BCJI], [770-BDZL]",1]
[{"$nulls":5},"System Documentation","GVRYSM7","No Systems Documentation, No OpenManage DVD Kit","[631-AACK]",1]
[{"$nulls":5},"SHIPPING","GIRGON7","PowerEdge R660XS Shipping EMEA1 (English/French/German/Spanish/Russian/Hebrew)","[340-DLRR]",1]
[{"$nulls":5},"Shipping Material","G3E81JA","PowerEdge R660xs, 8x2.5, Short Drive Shipping Material","[340-DFKP]",1]
[{"$nulls":5},"Regulatory","GE1ATIW","PowerEdge R660xs Label, CE and CCC Marking, for below 1300W PSU","[389-FBMD]",1]
[{"$nulls":5},"Shipping Box Labels - Standard","GDZ0XTY","Order Configuration Shipbox Label (Ship Date, Model, Processor Speed, HDD Size, RAM)","[293-10049]",1]
[{"$nulls":5},"Dell Services: Hardware Support","G2L3ABJ","Basic Next Business Day 36 Months, 36 Month(s)","[709-BBIL]",1]
[{"$nulls":5},"Dell Services:Extended Service","GUTGAE9","Prosupport Plus and 4Hr Mission Critical, 60 Month(s)","[865-BBNF], [865-BBNG]",1]
[{"$nulls":5},"Dell Services:Deployment Services",959563,"ProDeploy Plus Dell Server R Series 1U/2U","[683-19204], [683-19205], [706-12474]",1]
[{"$nulls":5},"Anti Theft Device & Asset Tagging","G2K1LTI","Asset Tag - ProSupport (Website, barcode, Onboard MacAddress)","[293-10025]",1]
[null,"Group 1","4242639.9.1","Management Domain: VxRail E660F - 4 Nodes (AZ1) ",4]
[{"$nulls":3},"VxRail E660/F/N - EMEA",1]
[{"$nulls":5},"Base","G0AKGOP","VxRail E660F, All Flash","[210-BBGQ], [329-BDWH]",1]
[{"$nulls":5},"Storage Deployment Module","G6G3RY9","vSAN Node","[379-BENB]",1]
[{"$nulls":5},"Operating System","GTZJM6E","VxRail Software 7.0.405 Factory Install","[384-BDHB], [634-BZQX]",1]
[{"$nulls":5},"VxRail configuration","G7HCORA","HCI System Software as part of Transformational License Agreement(TLA) and vSAN as part of VxRail","[379-BDUU]",1]
[{"$nulls":5},"Does this config require VCF software licenses?","GDMQ8NL","VCF","[379-BEWY]",1]
[{"$nulls":5},"VMware vSAN","G5UOPEY","Original Equipment Manufacturer ","[379-BEWY]",1]
[{"$nulls":5},"Chassis Configuration","G7ONJTM","2.5\" Chassis up to 10HDDs(SAS/SATA)including max of 4 Universal Drives,3PCIe Slots(vSAN Ent),2S","[321-BGUQ]",1]
[{"$nulls":5},"Bezel","G8S7MUQ","VxRail 1U Bezel V2","[325-BEBP]",1]
[{"$nulls":5},"Processor","GGMT2VC","Intel® Xeon® Gold 5320 2.2G, 26C/52T, 11.2GT/s, 39M Cache, Turbo, HT (185W) DDR4-2933","[338-CBXZ]",1]
[{"$nulls":5},"Additional Processor","GZO8H9D","Intel® Xeon® Gold 5320 2.2G, 26C/52T, 11.2GT/s, 39M Cache, Turbo, HT (185W) DDR4-2933","[338-CBXZ], [379-BDCO]",1]
[{"$nulls":5},"Memory DIMM Type and Speed","GR3CFNV","3200MT/s RDIMMs","[370-AEVR]",1]
[{"$nulls":5},"Memory Capacity","GFRC9EL","32GB RDIMM, 3200MT/s, Dual Rank, 16Gb BASE x8","[370-AGDS]",16]
[{"$nulls":5},"Hard Drives","GPWTK9J","1.6TB Enterprise NVMe Mixed Use AG Drive U.2 Gen4 with carrier","[400-BKGF]",2]
[{"$nulls":5},"Hard Drives","GS7WBQI","3.84TB SSD SATA Read Intensive 6Gbps 512 2.5in Hot-plug AG Drive, 1 DWPD","[400-AXSK]",6]
[{"$nulls":5},"PCIe Riser","G5HRD2Y","VxRail E660/F, Riser Config 0, 2CPU, 2A+3A, 2x16LP, 1x8LP","[330-BBVV]",1]
[{"$nulls":5},"OCP 3.0 Network Adapters","GAKY4CT","Broadcom 57504 Quad Port 10/25GbE,SFP28, OCP NIC 3.0","[540-BCRX]",1]
[{"$nulls":5},"Trusted Platform Module","GGX1VDO","Trusted Platform Module 2.0 V3","[461-AAIG]",1]
[{"$nulls":5},"Rack Rails","GSNQZP0","ReadyRails Sliding Rails With Cable Management Arm","[770-BDMT], [770-BECD]",1]
[{"$nulls":5},"Power Supply","GWT5F27","Dual, Hot-Plug, Power Supply Fault Tolerant Redundant (1+1), 1100W MM (100-240Vac) Titanium, NAF","[450-AKLF]",1]
[{"$nulls":5},"Power Cords",518051,"Rack Power Cord 2M (C13/C14 10A)","[450-AADY]",2]
[{"$nulls":5},"GPU/DPU Enablement","GWZQD4S","No GPU Enablement","[379-BDSR]",1]
[{"$nulls":5},"Dell Services: Hardware Support","GBHJ017","Parts Only Warranty 36 Months, 36 Month(s)","[709-BECW]",1]
[{"$nulls":5},"Dell Services:Extended Service","GWDRT0I","Prosupport Plus and 4Hr Mission Critical Onsite Service VSAN VCF on VxRail, 60 Month(s)","[199-BLKO], [199-BLKP]",1]
[{"$nulls":5},"Dell Services:Deployment Services","GOWD4C6","ProDeploy Plus: VCF on VxRail - Per Node Deploy","[683-24544], [706-12904]",1]
[{"$nulls":5},"Regulatory","G0GWKMD","PowerEdge R650 CE,CCC and BIS Marking on 2.5\" Chassis","[389-DZWK], [389-DZWN]",1]
[{"$nulls":5},"SAS/SATA/NVMe Backplane","GKJX6D9","SAS/SATA/NVMe Capable Backplane","[379-BDSW]",1]
[{"$nulls":5},"SHIPPING","GR2J1E7","E660/F/N Shipping, EMEA1","[631-ADCV]",1]
[{"$nulls":5},"Shipping Material","GSK7QEV","R650 Ship 4x3.5, 10x2.5, 8x2.5 NVMe","[340-CUQN]",1]
[{"$nulls":5},"Front Storage","GYEFL4N","10x2.5 Front Storage","[379-BEID]",1]
[{"$nulls":5},"Brand","GATWN48","VxRail E660F Branding","[329-BHKC]",1]
[{"$nulls":5},"Motherboard","GRXPG30","PowerEdge R650 Motherboard with Broadcom 5720 Dual Port 1Gb On-Board LOM, Ti","[329-BHMW]",1]
[{"$nulls":5},"Processor Thermal Configuration","G3KT0LF","Heatsink for 2 CPU configuration (CPU more than 165W)","[412-AAVM]",1]
[{"$nulls":5},"Memory Configuration Type","GH9QBEI","Performance Optimized","[370-AAIP]",1]
[{"$nulls":5},"RAID","GDG25FR","C35, No RAID","[780-BCQQ]",1]
[{"$nulls":5},"RAID/Internal Storage Controllers","GFC9AX8","Front HBA355 Rear Load (for Chassis up to 10 drives)","[405-AAXY], [750-ACFQ]",1]
[{"$nulls":5},"Boot optimized storage cards","GOK3C2G","BOSS-S2 controller card +  with 2 M.2 480GB (RAID 1)","[403-BCMB], [403-BCNP]",1]
[{"$nulls":5},"Embedded Systems Management","G4NWS93","iDRAC9, Enterprise 15G","[385-BBQV]",1]
[{"$nulls":5},"Group Manager","GTVA94K","iDRAC Group Manager, Disabled","[379-BCQY]",1]
[{"$nulls":5},"Password","GDOHU23","iDRAC,Legacy Password","[379-BCSG]",1]
[{"$nulls":5},"Systems Management Upgrades","GAP926M","DHCP, Zero Touch Configuration","[379-BCRB]",1]
[{"$nulls":5},"Fan","GKMQ9T4","4 High Performance Fans for 2 CPU","[750-ADIH]",1]
[{"$nulls":5},"Quick Sync","GI1FEZA","No Quick Sync","[350-BBXM]",1]
[{"$nulls":5},"System Documentation","GVRYSM7","No Systems Documentation, No OpenManage DVD Kit","[631-AACK]",1]
[{"$nulls":5},"Advanced System Configurations","G02CQJF","UEFI BIOS Boot Mode with GPT Partition, No Energy Star","[387-BBEY], [800-BBDM]",1]
[{"$nulls":5},"Luggage Tag","GC85RNY","E660F Luggage Tag","[350-BCFX]",1]
[{"$nulls":3},"VMware eOEM Licenses - EMEA",1]
[{"$nulls":5},"Base","GPJQ586","VxRail Software","[210-BDUK]",1]
[{"$nulls":5},"Does this config require VCF software licenses?","GDMQ8NL","VCF","[379-BEWY]",1]
[{"$nulls":5},"VMware vSAN","G5UOPEY","VxRail Vmware, VSAN Enterprise","[379-BEWY]",1]
[{"$nulls":5},"Additional Processor","GSEG289","Additional Processor Selected","[379-BDCO]",26]
[{"$nulls":5},"VMware vSAN Software Licenses","GXW31B0","VxRail VMware, vSAN Enterprise, 5 Years","[149-BBTC]",2]
[{"$nulls":5},"VMware Cloud Foundation Software Licenses","GPQG19X","VxRail VCF BYOLICENSE SOFTWARE","[379-BCRR], [384-BCTQ]",1]
[{"$nulls":5},"Sftwr Svcs - Perpetual (VP)","GW4MNVA","ProSupport Plus Mission Critical VxRail Sftwr Spt-Maint, 60 Month(s)","[487-BJPO]",1]
[{"$nulls":3},"Recoverpoint Services for VxRail - EMEA",1]
[{"$nulls":5},"Sftwr Svcs-Perpetual(VP)","GO4V0UH","ProSupport Plus Mission Critical RecoverPoint for VMs Software Support-Maintanance, 60 Month(s)","[487-BIPH]",1]
[{"$nulls":5},"Dell Services: Deployment Services",58267,"No Installation Service Selected (Contact Sales rep for more details)","[683-11870]",1]
[{"$nulls":5},"RecoverPoint for Virtual Machines","G1NHQMO","RecoverPoint for VMs-SWAAA","[210-BBOU]",1]
[{"$nulls":5},"RecoverPoint for VxRail","GH0B6KG","HCIA RecoverPoint for VMs for 1 node","[142-BBNV]",1]
[null,"Group 1","4242639.9.1","Management Domain: VxRail E660F - 4 Nodes (CPT) ",4]
[{"$nulls":3},"VxRail E660/F/N - EMEA",1]
[{"$nulls":5},"Base","G0AKGOP","VxRail E660F, All Flash","[210-BBGQ], [329-BDWH]",1]
[{"$nulls":5},"Storage Deployment Module","G6G3RY9","vSAN Node","[379-BENB]",1]
[{"$nulls":5},"Operating System","GTZJM6E","VxRail Software 7.0.405 Factory Install","[384-BDHB], [634-BZQX]",1]
[{"$nulls":5},"VxRail configuration","G7HCORA","HCI System Software as part of Transformational License Agreement(TLA) and vSAN as part of VxRail","[379-BDUU]",1]
[{"$nulls":5},"Does this config require VCF software licenses?","GDMQ8NL","VCF","[379-BEWY]",1]
[{"$nulls":5},"VMware vSAN","G5UOPEY","VxRail Vmware, VSAN Enterprise","[379-BEWY]",1]
[{"$nulls":5},"Chassis Configuration","G7ONJTM","2.5\" Chassis up to 10HDDs(SAS/SATA)including max of 4 Universal Drives,3PCIe Slots(vSAN Ent),2S","[321-BGUQ]",1]
[{"$nulls":5},"Bezel","G8S7MUQ","VxRail 1U Bezel V2","[325-BEBP]",1]
[{"$nulls":5},"Processor","GGMT2VC","Intel® Xeon® Gold 5320 2.2G, 26C/52T, 11.2GT/s, 39M Cache, Turbo, HT (185W) DDR4-2933","[338-CBXZ]",1]
[{"$nulls":5},"Additional Processor","GZO8H9D","Intel® Xeon® Gold 5320 2.2G, 26C/52T, 11.2GT/s, 39M Cache, Turbo, HT (185W) DDR4-2933","[338-CBXZ], [379-BDCO]",1]
[{"$nulls":5},"Memory DIMM Type and Speed","GR3CFNV","3200MT/s RDIMMs","[370-AEVR]",1]
[{"$nulls":5},"Memory Capacity","GFRC9EL","32GB RDIMM, 3200MT/s, Dual Rank, 16Gb BASE x8","[370-AGDS]",16]
[{"$nulls":5},"Hard Drives","GPWTK9J","1.6TB Enterprise NVMe Mixed Use AG Drive U.2 Gen4 with carrier","[400-BKGF]",2]
[{"$nulls":5},"Hard Drives","GS7WBQI","3.84TB SSD SATA Read Intensive 6Gbps 512 2.5in Hot-plug AG Drive, 1 DWPD","[400-AXSK]",6]
[{"$nulls":5},"PCIe Riser","G5HRD2Y","VxRail E660/F, Riser Config 0, 2CPU, 2A+3A, 2x16LP, 1x8LP","[330-BBVV]",1]
[{"$nulls":5},"OCP 3.0 Network Adapters","GAKY4CT","Broadcom 57504 Quad Port 10/25GbE,SFP28, OCP NIC 3.0","[540-BCRX]",1]
[{"$nulls":5},"Trusted Platform Module","GGX1VDO","Trusted Platform Module 2.0 V3","[461-AAIG]",1]
[{"$nulls":5},"Rack Rails","GSNQZP0","ReadyRails Sliding Rails With Cable Management Arm","[770-BDMT], [770-BECD]",1]
[{"$nulls":5},"Power Supply","GWT5F27","Dual, Hot-Plug, Power Supply Fault Tolerant Redundant (1+1), 1100W MM (100-240Vac) Titanium, NAF","[450-AKLF]",1]
[{"$nulls":5},"Power Cords",518051,"Rack Power Cord 2M (C13/C14 10A)","[450-AADY]",2]
[{"$nulls":5},"GPU/DPU Enablement","GWZQD4S","No GPU Enablement","[379-BDSR]",1]
[{"$nulls":5},"Dell Services: Hardware Support","GBHJ017","Parts Only Warranty 36 Months, 36 Month(s)","[709-BECW]",1]
[{"$nulls":5},"Dell Services:Extended Service","GWDRT0I","Prosupport Plus and 4Hr Mission Critical Onsite Service VSAN VCF on VxRail, 60 Month(s)","[199-BLKO], [199-BLKP]",1]
[{"$nulls":5},"Dell Services:Deployment Services","GOWD4C6","ProDeploy Plus: VCF on VxRail - Per Node Deploy","[683-24544], [706-12904]",1]
[{"$nulls":5},"Regulatory","G0GWKMD","PowerEdge R650 CE,CCC and BIS Marking on 2.5\" Chassis","[389-DZWK], [389-DZWN]",1]
[{"$nulls":5},"SAS/SATA/NVMe Backplane","GKJX6D9","SAS/SATA/NVMe Capable Backplane","[379-BDSW]",1]
[{"$nulls":5},"SHIPPING","GR2J1E7","E660/F/N Shipping, EMEA1","[631-ADCV]",1]
[{"$nulls":5},"Shipping Material","GSK7QEV","R650 Ship 4x3.5, 10x2.5, 8x2.5 NVMe","[340-CUQN]",1]
[{"$nulls":5},"Front Storage","GYEFL4N","10x2.5 Front Storage","[379-BEID]",1]
[{"$nulls":5},"Brand","GATWN48","VxRail E660F Branding","[329-BHKC]",1]
[{"$nulls":5},"Motherboard","GRXPG30","PowerEdge R650 Motherboard with Broadcom 5720 Dual Port 1Gb On-Board LOM, Ti","[329-BHMW]",1]
[{"$nulls":5},"Processor Thermal Configuration","G3KT0LF","Heatsink for 2 CPU configuration (CPU more than 165W)","[412-AAVM]",1]
[{"$nulls":5},"Memory Configuration Type","GH9QBEI","Performance Optimized","[370-AAIP]",1]
[{"$nulls":5},"RAID","GDG25FR","C35, No RAID","[780-BCQQ]",1]
[{"$nulls":5},"RAID/Internal Storage Controllers","GFC9AX8","Front HBA355 Rear Load (for Chassis up to 10 drives)","[405-AAXY], [750-ACFQ]",1]
[{"$nulls":5},"Boot optimized storage cards","GOK3C2G","BOSS-S2 controller card +  with 2 M.2 480GB (RAID 1)","[403-BCMB], [403-BCNP]",1]
[{"$nulls":5},"Embedded Systems Management","G4NWS93","iDRAC9, Enterprise 15G","[385-BBQV]",1]
[{"$nulls":5},"Group Manager","GTVA94K","iDRAC Group Manager, Disabled","[379-BCQY]",1]
[{"$nulls":5},"Password","GDOHU23","iDRAC,Legacy Password","[379-BCSG]",1]
[{"$nulls":5},"Systems Management Upgrades","GAP926M","DHCP, Zero Touch Configuration","[379-BCRB]",1]
[{"$nulls":5},"Fan","GKMQ9T4","4 High Performance Fans for 2 CPU","[750-ADIH]",1]
[{"$nulls":5},"Quick Sync","GI1FEZA","No Quick Sync","[350-BBXM]",1]
[{"$nulls":5},"System Documentation","GVRYSM7","No Systems Documentation, No OpenManage DVD Kit","[631-AACK]",1]
[{"$nulls":5},"Advanced System Configurations","G02CQJF","UEFI BIOS Boot Mode with GPT Partition, No Energy Star","[387-BBEY], [800-BBDM]",1]
[{"$nulls":5},"Luggage Tag","GC85RNY","E660F Luggage Tag","[350-BCFX]",1]
[{"$nulls":3},"VMware eOEM Licenses - EMEA",1]
[{"$nulls":5},"Base","GPJQ586","VxRail Software","[210-BDUK]",1]
[{"$nulls":5},"Does this config require VCF software licenses?","GDMQ8NL","VCF","[379-BEWY]",1]
[{"$nulls":5},"VMware vSAN","G5UOPEY","VxRail Vmware, VSAN Enterprise","[379-BEWY]",1]
[{"$nulls":5},"Additional Processor","GSEG289","Additional Processor Selected","[379-BDCO]",26]
[{"$nulls":5},"VMware vSAN Software Licenses","GXW31B0","VxRail VMware, vSAN Enterprise, 5 Years","[149-BBTC]",2]
[{"$nulls":5},"VMware Cloud Foundation Software Licenses","GPQG19X","VxRail VCF BYOLICENSE SOFTWARE","[379-BCRR], [384-BCTQ]",2]
[{"$nulls":5},"Sftwr Svcs - Perpetual (VP)","GW4MNVA","ProSupport Plus Mission Critical VxRail Sftwr Spt-Maint, 60 Month(s)","[487-BJPO]",1]
[{"$nulls":3},"Recoverpoint Services for VxRail - EMEA",1]
[{"$nulls":5},"Sftwr Svcs-Perpetual(VP)","GO4V0UH","ProSupport Plus Mission Critical RecoverPoint for VMs Software Support-Maintanance, 60 Month(s)","[487-BIPH]",1]
[{"$nulls":5},"Dell Services: Deployment Services",58267,"No Installation Service Selected (Contact Sales rep for more details)","[683-11870]",1]
[{"$nulls":5},"RecoverPoint for Virtual Machines","G1NHQMO","RecoverPoint for VMs-SWAAA","[210-BBOU]",1]
[{"$nulls":5},"RecoverPoint for VxRail","GH0B6KG","HCIA RecoverPoint for VMs for 1 node","[142-BBNV]",1]
[null,"Group 1","4242639.9.1","Management Domain: VxRail E660F - 4 Nodes (AZ2) ",4]
[{"$nulls":3},"VxRail E660/F/N - EMEA",1]
[{"$nulls":5},"Base","G0AKGOP","VxRail E660F, All Flash","[210-BBGQ], [329-BDWH]",1]
[{"$nulls":5},"Storage Deployment Module","G6G3RY9","vSAN Node","[379-BENB]",1]
[{"$nulls":5},"Operating System","GTZJM6E","VxRail Software 7.0.405 Factory Install","[384-BDHB], [634-BZQX]",1]
[{"$nulls":5},"VxRail configuration","G7HCORA","HCI System Software as part of Transformational License Agreement(TLA) and vSAN as part of VxRail","[379-BDUU]",1]
[{"$nulls":5},"Does this config require VCF software licenses?","GDMQ8NL","VCF","[379-BEWY]",1]
[{"$nulls":5},"VMware vSAN","G5UOPEY","VxRail Vmware, VSAN Enterprise","[379-BEWY]",1]
[{"$nulls":5},"Chassis Configuration","G7ONJTM","2.5\" Chassis up to 10HDDs(SAS/SATA)including max of 4 Universal Drives,3PCIe Slots(vSAN Ent),2S","[321-BGUQ]",1]
[{"$nulls":5},"Bezel","G8S7MUQ","VxRail 1U Bezel V2","[325-BEBP]",1]
[{"$nulls":5},"Processor","GGMT2VC","Intel® Xeon® Gold 5320 2.2G, 26C/52T, 11.2GT/s, 39M Cache, Turbo, HT (185W) DDR4-2933","[338-CBXZ]",1]
[{"$nulls":5},"Additional Processor","GZO8H9D","Intel® Xeon® Gold 5320 2.2G, 26C/52T, 11.2GT/s, 39M Cache, Turbo, HT (185W) DDR4-2933","[338-CBXZ], [379-BDCO]",1]
[{"$nulls":5},"Memory DIMM Type and Speed","GR3CFNV","3200MT/s RDIMMs","[370-AEVR]",1]
[{"$nulls":5},"Memory Capacity","GFRC9EL","32GB RDIMM, 3200MT/s, Dual Rank, 16Gb BASE x8","[370-AGDS]",16]
[{"$nulls":5},"Hard Drives","GPWTK9J","1.6TB Enterprise NVMe Mixed Use AG Drive U.2 Gen4 with carrier","[400-BKGF]",2]
[{"$nulls":5},"Hard Drives","GS7WBQI","3.84TB SSD SATA Read Intensive 6Gbps 512 2.5in Hot-plug AG Drive, 1 DWPD","[400-AXSK]",6]
[{"$nulls":5},"PCIe Riser","G5HRD2Y","VxRail E660/F, Riser Config 0, 2CPU, 2A+3A, 2x16LP, 1x8LP","[330-BBVV]",1]
[{"$nulls":5},"OCP 3.0 Network Adapters","GAKY4CT","Broadcom 57504 Quad Port 10/25GbE,SFP28, OCP NIC 3.0","[540-BCRX]",1]
[{"$nulls":5},"Trusted Platform Module","GGX1VDO","Trusted Platform Module 2.0 V3","[461-AAIG]",1]
[{"$nulls":5},"Rack Rails","GSNQZP0","ReadyRails Sliding Rails With Cable Management Arm","[770-BDMT], [770-BECD]",1]
[{"$nulls":5},"Power Supply","GWT5F27","Dual, Hot-Plug, Power Supply Fault Tolerant Redundant (1+1), 1100W MM (100-240Vac) Titanium, NAF","[450-AKLF]",1]
[{"$nulls":5},"Power Cords",518051,"Rack Power Cord 2M (C13/C14 10A)","[450-AADY]",2]
[{"$nulls":5},"GPU/DPU Enablement","GWZQD4S","No GPU Enablement","[379-BDSR]",1]
[{"$nulls":5},"Dell Services: Hardware Support","GBHJ017","Parts Only Warranty 36 Months, 36 Month(s)","[709-BECW]",1]
[{"$nulls":5},"Dell Services:Extended Service","GWDRT0I","Prosupport Plus and 4Hr Mission Critical Onsite Service VSAN VCF on VxRail, 60 Month(s)","[199-BLKO], [199-BLKP]",1]
[{"$nulls":5},"Dell Services:Deployment Services","GOWD4C6","ProDeploy Plus: VCF on VxRail - Per Node Deploy","[683-24544], [706-12904]",1]
[{"$nulls":5},"Regulatory","G0GWKMD","PowerEdge R650 CE,CCC and BIS Marking on 2.5\" Chassis","[389-DZWK], [389-DZWN]",1]
[{"$nulls":5},"SAS/SATA/NVMe Backplane","GKJX6D9","SAS/SATA/NVMe Capable Backplane","[379-BDSW]",1]
[{"$nulls":5},"SHIPPING","GR2J1E7","E660/F/N Shipping, EMEA1","[631-ADCV]",1]
[{"$nulls":5},"Shipping Material","GSK7QEV","R650 Ship 4x3.5, 10x2.5, 8x2.5 NVMe","[340-CUQN]",1]
[{"$nulls":5},"Front Storage","GYEFL4N","10x2.5 Front Storage","[379-BEID]",1]
[{"$nulls":5},"Brand","GATWN48","VxRail E660F Branding","[329-BHKC]",1]
[{"$nulls":5},"Motherboard","GRXPG30","PowerEdge R650 Motherboard with Broadcom 5720 Dual Port 1Gb On-Board LOM, Ti","[329-BHMW]",1]
[{"$nulls":5},"Processor Thermal Configuration","G3KT0LF","Heatsink for 2 CPU configuration (CPU more than 165W)","[412-AAVM]",1]
[{"$nulls":5},"Memory Configuration Type","GH9QBEI","Performance Optimized","[370-AAIP]",1]
[{"$nulls":5},"RAID","GDG25FR","C35, No RAID","[780-BCQQ]",1]
[{"$nulls":5},"RAID/Internal Storage Controllers","GFC9AX8","Front HBA355 Rear Load (for Chassis up to 10 drives)","[405-AAXY], [750-ACFQ]",1]
[{"$nulls":5},"Boot optimized storage cards","GOK3C2G","BOSS-S2 controller card +  with 2 M.2 480GB (RAID 1)","[403-BCMB], [403-BCNP]",1]
[{"$nulls":5},"Embedded Systems Management","G4NWS93","iDRAC9, Enterprise 15G","[385-BBQV]",1]
[{"$nulls":5},"Group Manager","GTVA94K","iDRAC Group Manager, Disabled","[379-BCQY]",1]
[{"$nulls":5},"Password","GDOHU23","iDRAC,Legacy Password","[379-BCSG]",1]
[{"$nulls":5},"Systems Management Upgrades","GAP926M","DHCP, Zero Touch Configuration","[379-BCRB]",1]
[{"$nulls":5},"Fan","GKMQ9T4","4 High Performance Fans for 2 CPU","[750-ADIH]",1]
[{"$nulls":5},"Quick Sync","GI1FEZA","No Quick Sync","[350-BBXM]",1]
[{"$nulls":5},"System Documentation","GVRYSM7","No Systems Documentation, No OpenManage DVD Kit","[631-AACK]",1]
[{"$nulls":5},"Advanced System Configurations","G02CQJF","UEFI BIOS Boot Mode with GPT Partition, No Energy Star","[387-BBEY], [800-BBDM]",1]
[{"$nulls":5},"Luggage Tag","GC85RNY","E660F Luggage Tag","[350-BCFX]",1]
[{"$nulls":3},"VMware eOEM Licenses - EMEA",1]
[{"$nulls":5},"Base","GPJQ586","VxRail Software","[210-BDUK]",1]
[{"$nulls":5},"Does this config require VCF software licenses?","GDMQ8NL","VCF","[379-BEWY]",1]
[{"$nulls":5},"VMware vSAN","G5UOPEY","VxRail Vmware, VSAN Enterprise","[379-BEWY]",1]
[{"$nulls":5},"Additional Processor","GSEG289","Additional Processor Selected","[379-BDCO]",26]
[{"$nulls":5},"VMware vSAN Software Licenses","GXW31B0","VxRail VMware, vSAN Enterprise, 5 Years","[149-BBTC]",2]
[{"$nulls":5},"VMware Cloud Foundation Software Licenses","GPQG19X","VxRail VCF BYOLICENSE SOFTWARE","[379-BCRR], [384-BCTQ]",2]
[{"$nulls":5},"Sftwr Svcs - Perpetual (VP)","GW4MNVA","ProSupport Plus Mission Critical VxRail Sftwr Spt-Maint, 60 Month(s)","[487-BJPO]",1]
[{"$nulls":3},"Recoverpoint Services for VxRail - EMEA",1]
[{"$nulls":5},"Sftwr Svcs-Perpetual(VP)","GO4V0UH","ProSupport Plus Mission Critical RecoverPoint for VMs Software Support-Maintanance, 60 Month(s)","[487-BIPH]",1]
[{"$nulls":5},"Dell Services: Deployment Services",58267,"No Installation Service Selected (Contact Sales rep for more details)","[683-11870]",1]
[{"$nulls":5},"RecoverPoint for Virtual Machines","G1NHQMO","RecoverPoint for VMs-SWAAA","[210-BBOU]",1]
[{"$nulls":5},"RecoverPoint for VxRail","GH0B6KG","HCIA RecoverPoint for VMs for 1 node","[142-BBNV]",1]
[null,"Group 1","4242639.9.1","Payload Domain: VxRail P670F - 5 Nodes (AZ1) ",5]
[{"$nulls":3},"VxRail P670F/N & V670F - EMEA",1]
[{"$nulls":5},"Base","GFE0B3S","VxRail P670F, All Flash","[210-BBGT], [329-BDWH]",1]
[{"$nulls":5},"Storage Deployment Module","GA63IQT","Dynamic Node","[379-BENC]",1]
[{"$nulls":5},"Operating System","G7ZKCOL","VxRail Software 7.0.450 Factory Install","[384-BDLF], [634-CCGB]",1]
[{"$nulls":5},"VxRail configuration","G0K5T74","HCI System Software as part of Transformational License Agreement(TLA)","[379-BEMZ]",1]
[{"$nulls":5},"Does this config require VCF software licenses?","GDMQ8NL","VCF","[379-BEWY]",1]
[{"$nulls":5},"Chassis Configuration","G6BKJNI","2.5\" Chassis with up to 24 HDDs (SAS/SATA/NVMe), 4x2.5\" Rear HDDs (SAS/SATA)","[321-BGYN]",1]
[{"$nulls":5},"Bezel","G0D3A6W","VxRail 2U Bezel V2","[325-BDYT]",1]
[{"$nulls":5},"Processor","G61X2LS","Intel® Xeon® Platinum 8358 2.6G, 32C/64T, 11.2GT/s, 48M Cache, Turbo, HT (250W) DDR4-3200","[338-CBCH]",1]
[{"$nulls":5},"Additional Processor","G629DFY","Intel® Xeon® Platinum 8358 2.6G, 32C/64T, 11.2GT/s, 48M Cache, Turbo, HT (250W) DDR4-3200","[338-CBCH], [379-BDCO]",1]
[{"$nulls":5},"Memory DIMM Type and Speed","GR3CFNV","3200MT/s RDIMMs","[370-AEVR]",1]
[{"$nulls":5},"Memory Capacity","GFRC9EL","32GB RDIMM, 3200MT/s, Dual Rank, 16Gb BASE x8","[370-AGDS]",16]
[{"$nulls":5},"Memory Capacity","GQC5KJW","64GB RDIMM, 3200MT/s, Dual Rank, 16Gb","[370-AEVP]",16]
[{"$nulls":5},"Hard Drives","GI1R734","No Hard Drive","[400-ABHL]",1]
[{"$nulls":5},"PCI Riser","GKVP92C","VxRail P670F, Riser Config 5, 2A+4B, 2x8FH, 2x16LP","[330-BBVY]",1]
[{"$nulls":5},"OCP 3.0 Network Adapters","GAKY4CT","Broadcom 57504 Quad Port 10/25GbE,SFP28, OCP NIC 3.0","[540-BCRX]",1]
[{"$nulls":5},"Fiber Channel Adapters","G7HFQLN","Emulex LPE 35002 Dual Port 32Gb Fibre Channel HBA, PCIe Low Profile","[406-BBMO]",1]
[{"$nulls":5},"Trusted Platform Module","GGX1VDO","Trusted Platform Module 2.0 V3","[461-AAIG]",1]
[{"$nulls":5},"Rack Rails","G25UX0L","ReadyRails Sliding Rails With Cable Management Arm","[770-BBBQ], [770-BDRQ]",1]
[{"$nulls":5},"Power Supply","GQE5JAW","Dual, Hot-Plug, Power Supply FTR, 1100W MM (100-240Vac) Titanium, Redundant (1+1)","[450-AKKS]",1]
[{"$nulls":5},"Power Cords",518051,"Rack Power Cord 2M (C13/C14 10A)","[450-AADY]",2]
[{"$nulls":5},"GPU ENABLEMENT","GWZQD4S","No GPU Enablement","[379-BDSR]",1]
[{"$nulls":5},"VMware vSAN","GCWLUO7","No vSAN","[379-BEWY]",1]
[{"$nulls":5},"Rear Storage","GD2LG5K","4x2.5  Rear Storage","[379-BDTB]",1]
[{"$nulls":5},"Server Accessories","GVYJO5Z","Fan Foam, HDD 2U","[750-ACOM]",1]
[{"$nulls":5},"Dell Services: Hardware Support","GBHJ017","Parts Only Warranty 36 Months, 36 Month(s)","[709-BECW]",1]
[{"$nulls":5},"Dell Services:Extended Service","GM4TG7U","Prosupport Plus and 4Hr Mission Critical No VSAN VCF on VxRail, 60 Month(s)","[199-BMIE], [199-BMIF]",1]
[{"$nulls":5},"Dell Services:Deployment Services","GOWD4C6","ProDeploy Plus: VCF on VxRail - Per Node Deploy","[683-24544], [706-12904]",1]
[{"$nulls":5},"Regulatory","G2L0H9K","PowerEdge R750 CE,CCC and BIS Marking on 2.5\" Chassis","[389-DZXU], [389-DZXV]",1]
[{"$nulls":5},"SAS/SATA/NVMe Backplane","GKJX6D9","SAS/SATA/NVMe Capable Backplane","[379-BDSW]",1]
[{"$nulls":5},"SHIPPING","GJ46ZF8","PV670/S670 Shipping, EMEA1","[631-ADCU]",1]
[{"$nulls":5},"Shipping Material","GT4H39R","PowerEdge R750 Shipping Material","[481-BBFG]",1]
[{"$nulls":5},"Front Storage","GBEZWO8","Chassis with up to 24x2.5\" Drives","[379-BDTF]",1]
[{"$nulls":5},"Brand","GBH74E8","VxRail P670F Branding","[329-BHKH]",1]
[{"$nulls":5},"Motherboard","GXETWB0","R750 Motherboard with Broadcom 5720 Dual Port 1Gb On-Board LOM","[329-BGJR]",1]
[{"$nulls":5},"Processor Thermal Configuration","G1Y5987","Heatsink for 2 CPU configuration (CPU greater than or equal to 165W)","[412-AAVB]",1]
[{"$nulls":5},"Memory Configuration Type","GH9QBEI","Performance Optimized","[370-AAIP]",1]
[{"$nulls":5},"RAID","GXTB459","VxRail RAID C44 ,Dynamic Node,PV670F","[780-BCRJ]",1]
[{"$nulls":5},"RAID/Internal Storage Controllers","G4G6IMP","Front HBA355 Rear Load (for 2.5\"x 24 SAS/SATA chassis)","[405-AAXY], [750-ADED]",1]
[{"$nulls":5},"Boot optimized storage cards","GYA7VZ6","BOSS-S2 controller card +  with 2 M.2 480GB (RAID 1) with Rear 4xBP","[403-BCMB], [470-AERS]",1]
[{"$nulls":5},"Embedded Systems Management","G4NWS93","iDRAC9, Enterprise 15G","[385-BBQV]",1]
[{"$nulls":5},"Group Manager","GTVA94K","iDRAC Group Manager, Disabled","[379-BCQY]",1]
[{"$nulls":5},"Password","GDOHU23","iDRAC,Legacy Password","[379-BCSG]",1]
[{"$nulls":5},"Systems Management Upgrades","GAP926M","DHCP, Zero Touch Configuration","[379-BCRB]",1]
[{"$nulls":5},"Fan","G8Z3VLX","Very High Performance Fan x6","[750-ADGJ]",1]
[{"$nulls":5},"Quick Sync","GCLNJM4","No Quick Sync","[350-BBYX]",1]
[{"$nulls":5},"System Documentation","GVRYSM7","No Systems Documentation, No OpenManage DVD Kit","[631-AACK]",1]
[{"$nulls":5},"Advanced System Configurations","G02CQJF","UEFI BIOS Boot Mode with GPT Partition, No Energy Star","[387-BBEY], [800-BBDM]",1]
[{"$nulls":5},"Luggage Tag","GR3WJMX","P670F Luggage Tag","[350-BCFZ]",1]
[{"$nulls":3},"VMware eOEM Licenses - EMEA",1]
[{"$nulls":5},"Base","GPJQ586","VxRail Software","[210-BDUK]",1]
[{"$nulls":5},"Does this config require VCF software licenses?","GDMQ8NL","VCF","[379-BEWY]",1]
[{"$nulls":5},"VMware vSAN","GCWLUO7","No vSAN","[379-BEWY]",1]
[{"$nulls":5},"Additional Processor","GSEG289","Additional Processor Selected","[379-BDCO]",32]
[{"$nulls":5},"VMware vSAN Software Licenses","GFPE3R9","No vSAN","[634-BZCO]",1]
[{"$nulls":5},"VMware Cloud Foundation Software Licenses","GPQG19X","VxRail VCF BYOLICENSE SOFTWARE","[379-BCRR], [384-BCTQ]",2]
[{"$nulls":5},"Sftwr Svcs - Perpetual (VP)","GW4MNVA","ProSupport Plus Mission Critical VxRail Sftwr Spt-Maint, 60 Month(s)","[487-BJPO]",1]
[{"$nulls":3},"Recoverpoint Services for VxRail - EMEA",1]
[{"$nulls":5},"Sftwr Svcs-Perpetual(VP)","GO4V0UH","ProSupport Plus Mission Critical RecoverPoint for VMs Software Support-Maintanance, 60 Month(s)","[487-BIPH]",1]
[{"$nulls":5},"Dell Services: Deployment Services",58267,"No Installation Service Selected (Contact Sales rep for more details)","[683-11870]",1]
[{"$nulls":5},"RecoverPoint for Virtual Machines","G1NHQMO","RecoverPoint for VMs-SWAAA","[210-BBOU]",1]
[{"$nulls":5},"RecoverPoint for VxRail","GH0B6KG","HCIA RecoverPoint for VMs for 1 node","[142-BBNV]",1]
[null,"Group 1","4242639.9.1","Payload Domain: VxRail P670F - 5 Nodes (AZ2) ",5]
[{"$nulls":3},"VxRail P670F/N & V670F - EMEA",1]
[{"$nulls":5},"Base","GFE0B3S","VxRail P670F, All Flash","[210-BBGT], [329-BDWH]",1]
[{"$nulls":5},"Storage Deployment Module","GA63IQT","Dynamic Node","[379-BENC]",1]
[{"$nulls":5},"Operating System","G7ZKCOL","VxRail Software 7.0.450 Factory Install","[384-BDLF], [634-CCGB]",1]
[{"$nulls":5},"VxRail configuration","G0K5T74","HCI System Software as part of Transformational License Agreement(TLA)","[379-BEMZ]",1]
[{"$nulls":5},"Does this config require VCF software licenses?","GDMQ8NL","VCF","[379-BEWY]",1]
[{"$nulls":5},"Chassis Configuration","G6BKJNI","2.5\" Chassis with up to 24 HDDs (SAS/SATA/NVMe), 4x2.5\" Rear HDDs (SAS/SATA)","[321-BGYN]",1]
[{"$nulls":5},"Bezel","G0D3A6W","VxRail 2U Bezel V2","[325-BDYT]",1]
[{"$nulls":5},"Processor","G61X2LS","Intel® Xeon® Platinum 8358 2.6G, 32C/64T, 11.2GT/s, 48M Cache, Turbo, HT (250W) DDR4-3200","[338-CBCH]",1]
[{"$nulls":5},"Additional Processor","G629DFY","Intel® Xeon® Platinum 8358 2.6G, 32C/64T, 11.2GT/s, 48M Cache, Turbo, HT (250W) DDR4-3200","[338-CBCH], [379-BDCO]",1]
[{"$nulls":5},"Memory DIMM Type and Speed","GR3CFNV","3200MT/s RDIMMs","[370-AEVR]",1]
[{"$nulls":5},"Memory Capacity","GFRC9EL","32GB RDIMM, 3200MT/s, Dual Rank, 16Gb BASE x8","[370-AGDS]",16]
[{"$nulls":5},"Memory Capacity","GQC5KJW","64GB RDIMM, 3200MT/s, Dual Rank, 16Gb","[370-AEVP]",16]
[{"$nulls":5},"Hard Drives","GI1R734","No Hard Drive","[400-ABHL]",1]
[{"$nulls":5},"PCI Riser","GKVP92C","VxRail P670F, Riser Config 5, 2A+4B, 2x8FH, 2x16LP","[330-BBVY]",1]
[{"$nulls":5},"OCP 3.0 Network Adapters","GAKY4CT","Broadcom 57504 Quad Port 10/25GbE,SFP28, OCP NIC 3.0","[540-BCRX]",1]
[{"$nulls":5},"Fiber Channel Adapters","G7HFQLN","Emulex LPE 35002 Dual Port 32Gb Fibre Channel HBA, PCIe Low Profile","[406-BBMO]",1]
[{"$nulls":5},"Trusted Platform Module","GGX1VDO","Trusted Platform Module 2.0 V3","[461-AAIG]",1]
[{"$nulls":5},"Rack Rails","G25UX0L","ReadyRails Sliding Rails With Cable Management Arm","[770-BBBQ], [770-BDRQ]",1]
[{"$nulls":5},"Power Supply","GQE5JAW","Dual, Hot-Plug, Power Supply FTR, 1100W MM (100-240Vac) Titanium, Redundant (1+1)","[450-AKKS]",1]
[{"$nulls":5},"Power Cords",518051,"Rack Power Cord 2M (C13/C14 10A)","[450-AADY]",2]
[{"$nulls":5},"GPU ENABLEMENT","GWZQD4S","No GPU Enablement","[379-BDSR]",1]
[{"$nulls":5},"VMware vSAN","GCWLUO7","No vSAN","[379-BEWY]",1]
[{"$nulls":5},"Rear Storage","GD2LG5K","4x2.5  Rear Storage","[379-BDTB]",1]
[{"$nulls":5},"Server Accessories","GVYJO5Z","Fan Foam, HDD 2U","[750-ACOM]",1]
[{"$nulls":5},"Dell Services: Hardware Support","GBHJ017","Parts Only Warranty 36 Months, 36 Month(s)","[709-BECW]",1]
[{"$nulls":5},"Dell Services:Extended Service","GM4TG7U","Prosupport Plus and 4Hr Mission Critical No VSAN VCF on VxRail, 60 Month(s)","[199-BMIE], [199-BMIF]",1]
[{"$nulls":5},"Dell Services:Deployment Services","GOWD4C6","ProDeploy Plus: VCF on VxRail - Per Node Deploy","[683-24544], [706-12904]",1]
[{"$nulls":5},"Regulatory","G2L0H9K","PowerEdge R750 CE,CCC and BIS Marking on 2.5\" Chassis","[389-DZXU], [389-DZXV]",1]
[{"$nulls":5},"SAS/SATA/NVMe Backplane","GKJX6D9","SAS/SATA/NVMe Capable Backplane","[379-BDSW]",1]
[{"$nulls":5},"SHIPPING","GJ46ZF8","PV670/S670 Shipping, EMEA1","[631-ADCU]",1]
[{"$nulls":5},"Shipping Material","GT4H39R","PowerEdge R750 Shipping Material","[481-BBFG]",1]
[{"$nulls":5},"Front Storage","GBEZWO8","Chassis with up to 24x2.5\" Drives","[379-BDTF]",1]
[{"$nulls":5},"Brand","GBH74E8","VxRail P670F Branding","[329-BHKH]",1]
[{"$nulls":5},"Motherboard","GXETWB0","R750 Motherboard with Broadcom 5720 Dual Port 1Gb On-Board LOM","[329-BGJR]",1]
[{"$nulls":5},"Processor Thermal Configuration","G1Y5987","Heatsink for 2 CPU configuration (CPU greater than or equal to 165W)","[412-AAVB]",1]
[{"$nulls":5},"Memory Configuration Type","GH9QBEI","Performance Optimized","[370-AAIP]",1]
[{"$nulls":5},"RAID","GXTB459","VxRail RAID C44 ,Dynamic Node,PV670F","[780-BCRJ]",1]
[{"$nulls":5},"RAID/Internal Storage Controllers","G4G6IMP","Front HBA355 Rear Load (for 2.5\"x 24 SAS/SATA chassis)","[405-AAXY], [750-ADED]",1]
[{"$nulls":5},"Boot optimized storage cards","GYA7VZ6","BOSS-S2 controller card +  with 2 M.2 480GB (RAID 1) with Rear 4xBP","[403-BCMB], [470-AERS]",1]
[{"$nulls":5},"Embedded Systems Management","G4NWS93","iDRAC9, Enterprise 15G","[385-BBQV]",1]
[{"$nulls":5},"Group Manager","GTVA94K","iDRAC Group Manager, Disabled","[379-BCQY]",1]
[{"$nulls":5},"Password","GDOHU23","iDRAC,Legacy Password","[379-BCSG]",1]
[{"$nulls":5},"Systems Management Upgrades","GAP926M","DHCP, Zero Touch Configuration","[379-BCRB]",1]
[{"$nulls":5},"Fan","G8Z3VLX","Very High Performance Fan x6","[750-ADGJ]",1]
[{"$nulls":5},"Quick Sync","GCLNJM4","No Quick Sync","[350-BBYX]",1]
[{"$nulls":5},"System Documentation","GVRYSM7","No Systems Documentation, No OpenManage DVD Kit","[631-AACK]",1]
[{"$nulls":5},"Advanced System Configurations","G02CQJF","UEFI BIOS Boot Mode with GPT Partition, No Energy Star","[387-BBEY], [800-BBDM]",1]
[{"$nulls":5},"Luggage Tag","GR3WJMX","P670F Luggage Tag","[350-BCFZ]",1]
[{"$nulls":3},"VMware eOEM Licenses - EMEA",1]
[{"$nulls":5},"Base","GPJQ586","VxRail Software","[210-BDUK]",1]
[{"$nulls":5},"Does this config require VCF software licenses?","GDMQ8NL","VCF","[379-BEWY]",1]
[{"$nulls":5},"VMware vSAN","GCWLUO7","No vSAN","[379-BEWY]",1]
[{"$nulls":5},"Additional Processor","GSEG289","Additional Processor Selected","[379-BDCO]",32]
[{"$nulls":5},"VMware vSAN Software Licenses","GFPE3R9","No vSAN","[634-BZCO]",1]
[{"$nulls":5},"VMware Cloud Foundation Software Licenses","GPQG19X","VxRail VCF BYOLICENSE SOFTWARE","[379-BCRR], [384-BCTQ]",2]
[{"$nulls":5},"Sftwr Svcs - Perpetual (VP)","GW4MNVA","ProSupport Plus Mission Critical VxRail Sftwr Spt-Maint, 60 Month(s)","[487-BJPO]",1]
[{"$nulls":3},"Recoverpoint Services for VxRail - EMEA",1]
[{"$nulls":5},"Sftwr Svcs-Perpetual(VP)","GO4V0UH","ProSupport Plus Mission Critical RecoverPoint for VMs Software Support-Maintanance, 60 Month(s)","[487-BIPH]",1]
[{"$nulls":5},"Dell Services: Deployment Services",58267,"No Installation Service Selected (Contact Sales rep for more details)","[683-11870]",1]
[{"$nulls":5},"RecoverPoint for Virtual Machines","G1NHQMO","RecoverPoint for VMs-SWAAA","[210-BBOU]",1]
[{"$nulls":5},"RecoverPoint for VxRail","GH0B6KG","HCIA RecoverPoint for VMs for 1 node","[142-BBNV]",1]
[null,"Group 1","4242639.9.1","Payload Domain: VxRail P670F - 5 Nodes (CPT) ",5]
[{"$nulls":3},"VxRail P670F/N & V670F - EMEA",1]
[{"$nulls":5},"Base","GFE0B3S","VxRail P670F, All Flash","[210-BBGT], [329-BDWH]",1]
[{"$nulls":5},"Storage Deployment Module","GA63IQT","Dynamic Node","[379-BENC]",1]
[{"$nulls":5},"Operating System","G7ZKCOL","VxRail Software 7.0.450 Factory Install","[384-BDLF], [634-CCGB]",1]
[{"$nulls":5},"VxRail configuration","G0K5T74","HCI System Software as part of Transformational License Agreement(TLA)","[379-BEMZ]",1]
[{"$nulls":5},"Does this config require VCF software licenses?","GDMQ8NL","VCF","[379-BEWY]",1]
[{"$nulls":5},"Chassis Configuration","G6BKJNI","2.5\" Chassis with up to 24 HDDs (SAS/SATA/NVMe), 4x2.5\" Rear HDDs (SAS/SATA)","[321-BGYN]",1]
[{"$nulls":5},"Bezel","G0D3A6W","VxRail 2U Bezel V2","[325-BDYT]",1]
[{"$nulls":5},"Processor","G61X2LS","Intel® Xeon® Platinum 8358 2.6G, 32C/64T, 11.2GT/s, 48M Cache, Turbo, HT (250W) DDR4-3200","[338-CBCH]",1]
[{"$nulls":5},"Additional Processor","G629DFY","Intel® Xeon® Platinum 8358 2.6G, 32C/64T, 11.2GT/s, 48M Cache, Turbo, HT (250W) DDR4-3200","[338-CBCH], [379-BDCO]",1]
[{"$nulls":5},"Memory DIMM Type and Speed","GR3CFNV","3200MT/s RDIMMs","[370-AEVR]",1]
[{"$nulls":5},"Memory Capacity","GFRC9EL","32GB RDIMM, 3200MT/s, Dual Rank, 16Gb BASE x8","[370-AGDS]",16]
[{"$nulls":5},"Memory Capacity","GQC5KJW","64GB RDIMM, 3200MT/s, Dual Rank, 16Gb","[370-AEVP]",16]
[{"$nulls":5},"Hard Drives","GI1R734","No Hard Drive","[400-ABHL]",1]
[{"$nulls":5},"PCI Riser","GKVP92C","VxRail P670F, Riser Config 5, 2A+4B, 2x8FH, 2x16LP","[330-BBVY]",1]
[{"$nulls":5},"OCP 3.0 Network Adapters","GAKY4CT","Broadcom 57504 Quad Port 10/25GbE,SFP28, OCP NIC 3.0","[540-BCRX]",1]
[{"$nulls":5},"Fiber Channel Adapters","G7HFQLN","Emulex LPE 35002 Dual Port 32Gb Fibre Channel HBA, PCIe Low Profile","[406-BBMO]",1]
[{"$nulls":5},"Trusted Platform Module","GGX1VDO","Trusted Platform Module 2.0 V3","[461-AAIG]",1]
[{"$nulls":5},"Rack Rails","G25UX0L","ReadyRails Sliding Rails With Cable Management Arm","[770-BBBQ], [770-BDRQ]",1]
[{"$nulls":5},"Power Supply","GQE5JAW","Dual, Hot-Plug, Power Supply FTR, 1100W MM (100-240Vac) Titanium, Redundant (1+1)","[450-AKKS]",1]
[{"$nulls":5},"Power Cords",518051,"Rack Power Cord 2M (C13/C14 10A)","[450-AADY]",2]
[{"$nulls":5},"GPU ENABLEMENT","GWZQD4S","No GPU Enablement","[379-BDSR]",1]
[{"$nulls":5},"VMware vSAN","GCWLUO7","No vSAN","[379-BEWY]",1]
[{"$nulls":5},"Rear Storage","GD2LG5K","4x2.5  Rear Storage","[379-BDTB]",1]
[{"$nulls":5},"Server Accessories","GVYJO5Z","Fan Foam, HDD 2U","[750-ACOM]",1]
[{"$nulls":5},"Dell Services: Hardware Support","GBHJ017","Parts Only Warranty 36 Months, 36 Month(s)","[709-BECW]",1]
[{"$nulls":5},"Dell Services:Extended Service","GM4TG7U","Prosupport Plus and 4Hr Mission Critical No VSAN VCF on VxRail, 60 Month(s)","[199-BMIE], [199-BMIF]",1]
[{"$nulls":5},"Dell Services:Deployment Services","GOWD4C6","ProDeploy Plus: VCF on VxRail - Per Node Deploy","[683-24544], [706-12904]",1]
[{"$nulls":5},"Regulatory","G2L0H9K","PowerEdge R750 CE,CCC and BIS Marking on 2.5\" Chassis","[389-DZXU], [389-DZXV]",1]
[{"$nulls":5},"SAS/SATA/NVMe Backplane","GKJX6D9","SAS/SATA/NVMe Capable Backplane","[379-BDSW]",1]
[{"$nulls":5},"SHIPPING","GJ46ZF8","PV670/S670 Shipping, EMEA1","[631-ADCU]",1]
[{"$nulls":5},"Shipping Material","GT4H39R","PowerEdge R750 Shipping Material","[481-BBFG]",1]
[{"$nulls":5},"Front Storage","GBEZWO8","Chassis with up to 24x2.5\" Drives","[379-BDTF]",1]
[{"$nulls":5},"Brand","GBH74E8","VxRail P670F Branding","[329-BHKH]",1]
[{"$nulls":5},"Motherboard","GXETWB0","R750 Motherboard with Broadcom 5720 Dual Port 1Gb On-Board LOM","[329-BGJR]",1]
[{"$nulls":5},"Processor Thermal Configuration","G1Y5987","Heatsink for 2 CPU configuration (CPU greater than or equal to 165W)","[412-AAVB]",1]
[{"$nulls":5},"Memory Configuration Type","GH9QBEI","Performance Optimized","[370-AAIP]",1]
[{"$nulls":5},"RAID","GXTB459","VxRail RAID C44 ,Dynamic Node,PV670F","[780-BCRJ]",1]
[{"$nulls":5},"RAID/Internal Storage Controllers","G4G6IMP","Front HBA355 Rear Load (for 2.5\"x 24 SAS/SATA chassis)","[405-AAXY], [750-ADED]",1]
[{"$nulls":5},"Boot optimized storage cards","GYA7VZ6","BOSS-S2 controller card +  with 2 M.2 480GB (RAID 1) with Rear 4xBP","[403-BCMB], [470-AERS]",1]
[{"$nulls":5},"Embedded Systems Management","G4NWS93","iDRAC9, Enterprise 15G","[385-BBQV]",1]
[{"$nulls":5},"Group Manager","GTVA94K","iDRAC Group Manager, Disabled","[379-BCQY]",1]
[{"$nulls":5},"Password","GDOHU23","iDRAC,Legacy Password","[379-BCSG]",1]
[{"$nulls":5},"Systems Management Upgrades","GAP926M","DHCP, Zero Touch Configuration","[379-BCRB]",1]
[{"$nulls":5},"Fan","G8Z3VLX","Very High Performance Fan x6","[750-ADGJ]",1]
[{"$nulls":5},"Quick Sync","GCLNJM4","No Quick Sync","[350-BBYX]",1]
[{"$nulls":5},"System Documentation","GVRYSM7","No Systems Documentation, No OpenManage DVD Kit","[631-AACK]",1]
[{"$nulls":5},"Advanced System Configurations","G02CQJF","UEFI BIOS Boot Mode with GPT Partition, No Energy Star","[387-BBEY], [800-BBDM]",1]
[{"$nulls":5},"Luggage Tag","GR3WJMX","P670F Luggage Tag","[350-BCFZ]",1]
[{"$nulls":3},"VMware eOEM Licenses - EMEA",1]
[{"$nulls":5},"Base","GPJQ586","VxRail Software","[210-BDUK]",1]
[{"$nulls":5},"Does this config require VCF software licenses?","GDMQ8NL","VCF","[379-BEWY]",1]
[{"$nulls":5},"VMware vSAN","GCWLUO7","No vSAN","[379-BEWY]",1]
[{"$nulls":5},"Additional Processor","GSEG289","Additional Processor Selected","[379-BDCO]",32]
[{"$nulls":5},"VMware vSAN Software Licenses","GFPE3R9","No vSAN","[634-BZCO]",1]
[{"$nulls":5},"VMware Cloud Foundation Software Licenses","GPQG19X","VxRail VCF BYOLICENSE SOFTWARE","[379-BCRR], [384-BCTQ]",2]
[{"$nulls":5},"Sftwr Svcs - Perpetual (VP)","GW4MNVA","ProSupport Plus Mission Critical VxRail Sftwr Spt-Maint, 60 Month(s)","[487-BJPO]",1]
[{"$nulls":3},"Recoverpoint Services for VxRail - EMEA",1]
[{"$nulls":5},"Sftwr Svcs-Perpetual(VP)","GO4V0UH","ProSupport Plus Mission Critical RecoverPoint for VMs Software Support-Maintanance, 60 Month(s)","[487-BIPH]",1]
[{"$nulls":5},"Dell Services: Deployment Services",58267,"No Installation Service Selected (Contact Sales rep for more details)","[683-11870]",1]
[{"$nulls":5},"RecoverPoint for Virtual Machines","G1NHQMO","RecoverPoint for VMs-SWAAA","[210-BBOU]",1]
[{"$nulls":5},"RecoverPoint for VxRail","GH0B6KG","HCIA RecoverPoint for VMs for 1 node","[142-BBNV]",1]
[null,"Group 1","4242639.9.1","1. S3048-ON – Full Configuration - [DSDNS3048] (Mgmt Switches) ",3]
[{"$nulls":5},"Operating System","OS10E","OS10 Enterprise, S3048-ON","[634-BIXD]",1]
[{"$nulls":5},"Base",546973,"Dell Networking S3048-ON, 48x 1GbE, 4x SFP+ 10GbE ports,  Stacking, IO to PSU air, 1x AC PSU, NO OS","[210-AEDN]",1]
[{"$nulls":5},"System Documentation",546977,"S3048-ON User Documentation","[634-BDXK]",1]
[{"$nulls":5},"Power Cords",527294,"Rack Power Cord 2M, C13/C14, 12A","[450-AART]",1]
[{"$nulls":5},"Optics","G50DQNX","Dell Networking, Transceiver, SFP+, 10GbE, SR, 850nm Wavelength, 300m Reach","[407-BCZR]",1]
[{"$nulls":5},"Order Information",159009,"Enterprise Order - EMEA","[800-11671]",1]
[{"$nulls":5},"Dell Services: Deployment Services",959528,"ProDeploy Plus Dell Networking S Series 3XXX Switch","[683-19368], [683-19369], [706-12528]",1]
[{"$nulls":5},"Base warranty",935624,"1Yr Return to Depot - Minimum Warranty","[709-13047], [709-13048], [709-13051], [709-13052]",1]
[{"$nulls":5},"Support Services",935840,"5Yr ProSupport Plus and 4hr Mission Critical","[528-10337], [710-73917], [710-73921]",1]
[null,"Group 1","4242639.9.1","CS_AR3300 *SAF Only* NetShelter SX 42U/600mm/1200mm Enclosure with Roof and Sides Black ",3]
[null,"Group 1","4242639.9.1","CS_AP8853 *SAF Only* Rack PDU 2G, Metered, ZeroU, 32A, 230V, (36) C13 & (6) C19 ",6]
[null,"Group 1","4242639.9.1","C2G - Cat6 Ethernet (RJ-45) UTP Snagless Cable - Black - 5m ",45]
[null,"Group 1","4242639.9.1","EMC_POWERSTORET_GEN2_EMEA_2 (AZ1) ",1]
[{"$nulls":3},"Dell PowerStore 1200 T - EMEA",1]
[{"$nulls":5},"PowerStore 1200","GABW73H","PowerStore 1200T Base Dell Customer Racked TLA","[210-BCZK]",1]
[{"$nulls":5},"Memory Capacity","G58PSGD","384GB Appliance DIMM (192GB Per Node)","[370-AEZP]",1]
[{"$nulls":5},"DRR (Used for Internal Data Tracking)","GCUT7NJ",0.12569444444444444,"[379-BEIQ]",1]
[{"$nulls":5},"Drives","GT6URWQ","15.36TB NVMe SSD (High Capacity Array) TLA","[400-BQGF]",15]
[{"$nulls":5},"Operating Environment","GLC6HFV","TLA HW Only Order","[379-BDUU]",1]
[{"$nulls":5},"4 Port Mezz Cards","GP59QJZ","25GBE Optical 4 Port Card Pair (SFPs not included)","[406-BBOO]",1]
[{"$nulls":5},"Optional Appliance IO Module","GSCX3RP","32GB FC 4 Port IO Module Pair (SFPs included)","[565-BBJS]",1]
[{"$nulls":5},"Power Supply","GOQ271R","Dual 1800W (200-240V) Lot 9 Power Supply , includes C13/C14 Power Cords","[450-BBBJ]",1]
[{"$nulls":5},"Cable Pairs","GFKM8N4","3M Passive 25G Twinax Cable QTY 2","[470-ADUI]",4]
[{"$nulls":5},"Install Kits","GP49UY5","PowerStore Base Enclosure Install Kit","[343-BBTN]",1]
[{"$nulls":5},"NVRAM Caching Device","G0A32UK","PowerStore NVRAM FIPS QTY 2","[400-BOBK]",1]
[{"$nulls":5},"Dell Services: Hardware Support","G6JLC01","Parts Only Warranty 36Months, 36 Month(s)","[709-BDKZ]",1]
[{"$nulls":5},"Dell Services: Extended Service","GM6395C","Prosupport Plus and 4Hr Mission Critical, 60 Month(s)","[199-BJJO], [199-BJJP]",1]
[{"$nulls":5},"Storage Configuration","GIY80C2","Single Appliance","[800-BBQV]",1]
[{"$nulls":5},"Dell Services:Deployment Services","G4YRE2B","ProDeploy Plus for PowerStore 1xxx T","[683-23387], [706-12528]",1]
[{"$nulls":5},"Dell Services:Additional Deployment Services","GY4R9AF","ProDeploy Plus Add-On for PowerStore Remote Replication (Requires ProDeploy Plus)","[519-10199]",1]
[{"$nulls":5},"Dell Services:Additional Deployment Services","GG6179R","ProDeploy Plus Add-On for PowerStore Local Protection (Requires ProDeploy Plus)","[519-10194]",1]
[{"$nulls":5},"Data Migration Services","G7WJPUC","Data Migration Services: Remote Virtual V2V Migration 101 Plus VMs (Per VM)","[519-12227]",135]
[{"$nulls":3},"Metro node for PowerStore  EMEA",2]
[{"$nulls":5},"Dell EMC metro node","G7ZD5CJ","Metro node Base Configuration","[210-AXRR], [321-BCYJ], [329-BDMR], [330-BBGN], [350-BBKB], [350-BCCT], [370-AAIP], [370-AEVR], [379-BCQW], [379-BCQY], [379-BDCO], [384-BBQJ], [385-BBKT], [405-AACD], [429-ABBF], [450-AAGG], [450-AJSC], [461-AADZ], [540-BBVO], [555-BCKP], [605-BBFN], [623-BBDW], [631-AACK], [631-ACTH], [770-BCIO], [780-BCDM], [800-BBDM]",1]
[{"$nulls":5},"Fibre Channel Adapters","G7HFQLN","Emulex LPE 35002 Dual Port 32Gb Fibre Channel HBA, PCIe Low Profile","[406-BBMO]",2]
[{"$nulls":5},"Hard Drives","G3ZJM0K","480GB SSD SATA Read Intensive 6Gbps 512 2.5in Hot-plug AG Drive, 1 DWPD","[400-AXTV]",1]
[{"$nulls":5},"Optics","G0FVJIE","SFP+ SR Optic, 10GbE, for all SFP+ ports except high temp validation warning cards","[407-BCBE]",2]
[{"$nulls":5},"Memory DIMM","GQ3BS0I","16GB RDIMM, 3200MT/s, Dual Rank","[370-AEVQ]",4]
[{"$nulls":5},"Processor","GS1G2MP","Intel Xeon Silver 4208 2.1G, 8C/16T, 9.6GT/s, 11M Cache, Turbo, HT (85W) DDR4-2400","[338-BSWX]",2]
[{"$nulls":5},"Processor Thermal Configuration",5099793,"Standard Heatsink for 2 CPU","[370-ABWE], [412-AAIQ], [412-AAIQ]",1]
[{"$nulls":5},"Brand Kit","GKHZXQ0","Bezel and Luggage Tag for PowerStore","[325-BDZP], [350-BCDY]",1]
[{"$nulls":5},"Cable Management Arm Kit","G4PAORU","CMA KIT (PWR,LCOM,MGMT Cables Included)","[470-AENQ]",1]
[{"$nulls":5},"Dell Services: Hardware Support","G0NZD1S","Basic Next Business Day 36Months, 36 Month(s)","[709-BDRR]",1]
[{"$nulls":5},"Dell Services: Extended Service","GBUE8WV","ProSupport Plus and 4Hr Mission Critical, 60 Month(s)","[199-BJXL], [199-BJXM]",1]
[{"$nulls":5},"Metro node Operating System","GFQ6SOY","Metro node Operating System","[528-CNOH]",1]
[{"$nulls":5},"Local Capacity License","GCSM8YX","Local 10TB Capacity License","[528-CNPF]",1]
[{"$nulls":5},"Software Services - Metro node Local Base Capacity","GNX103T","ProSupport Plus Mission Critical metro node Local Base Incl 10TB Software Support-Maint, 60 Month(s)","[487-BGNT]",1]
[{"$nulls":5},"Dell Services: Deployment Services","G8QMLNH","ProDeploy Plus for Metro Node Single Node  Deployment","[683-26310], [706-12529]",1]
[{"$nulls":5},"Shipping Material","GQPW7FK","PowerEdge R640 x8 Drive Shipping Material","[340-COPS]",1]
[{"$nulls":5},"Regulatory","G27VF4L","PowerEdge R640 CE,CCC,BIS Marking","[389-DTIV]",1]
[{"$nulls":5},"Shipping","GBIHPJ4","Metro node Shipping EMEA1","[340-CUXV]",1]
[{"$nulls":3},"Metro node Software for PowerStore  EMEA",1]
[{"$nulls":5},"Metro node Software","GR8PWBT","Metro node Software","[210-AYIY]",1]
[{"$nulls":5},"Hardware Selection","GA217I9","PowerStore","[800-BBQV]",1]
[{"$nulls":5},"Metro node Powerstore Frame License","GGJY7DR","Metro node PowerStore 1K METRO FB SW","[528-CNNT]",1]
[{"$nulls":5},"Software Services : Perpetual (VP)","G2TX1H3","ProSupport Plus Mission Critical metro node Software Support-Maintenance, 60 Month(s)","[487-BGJY]",1]
[{"$nulls":3},"Metro node Deployment Services - EMEA",1]
[{"$nulls":5},"Metro node Deployment Services","G5L4CX2","Metro node Deployment Services","[210-BBCB]",1]
[{"$nulls":5},"Add-On Services for ProDeploy","GFGWRS5","ProDeploy Plus Add-On:  Metro Node Witness Module (Requires ProDeploy Plus)","[519-12568]",1]
[{"$nulls":3},"Dell EMC AppSync for PowerStore - EMEA",1]
[{"$nulls":5},"Appsync for PowerStore","GB81KRV","AppSync for PowerStore","[210-BEGM]",1]
[{"$nulls":5},"Deployment Services",57261,"No Installation Service Selected (Contact Sales rep for more details)","[683-11930]",1]
[{"$nulls":5},"AppSync Software","GQ70RAI","AppSync Str Pk for PowerStore","[528-BYHF]",1]
[{"$nulls":5},"Sftwr Svcs - Perpetual","G5F3N98","ProSupport Plus Mission Critical Appsync for PowerStore Sftwr Spt-Maint, 60 Month(s)","[487-BJQM]",1]
[{"$nulls":3},"Connectrix DS-6620B MidRange Cosell",2]
[{"$nulls":5},"Connectrix DS-6620B","GAWJUZ0","DS-6620B 24P/48P V2 switch (FOS 9.0 min) w/front-to-rear airflow (includes 24x32Gb SFPs a","[210-AZLG]",1]
[{"$nulls":5},"Dell Services: Hardware Support","G5COX36","Parts Only Warranty 36Months, 36 Month(s)","[709-BDSY]",1]
[{"$nulls":5},"Dell Services: Extended Service","GTWKL3Y","ProSupport Plus and 4Hr Mission Critical, 60 Month(s)","[199-BJSW], [199-BJSX]",1]
[{"$nulls":5},"Dell Services: Deployment Services","G26UVJX","ProDeploy Plus Connectrix Fibre Channel Switch (up to 4 new hosts)","[683-23121], [683-23122], [706-12472]",1]
[{"$nulls":5},"MultiMode Fiber LC/LC patch cables","GBFV6RW","OM4 LC/LC Multi Mode Fiber Cable (optics required), 5 Meter","[407-BCQM]",12]
[{"$nulls":5},"MultiMode Fiber LC/LC patch cables","G9L1FGK","OM4 LC/LC Multi Mode Fiber Cable (optics required), 10 Meter","[407-BCQH]",12]
[{"$nulls":5},"Power Cords","GN3XZY2","QTY 2 Connectrix C14-TO-C13 3M INTERNAL CAB POWER CORDS-B","[450-ABLX]",1]
[null,"Group 1","4242639.9.1","EMC_POWERSTORET_GEN2_EMEA_2 (AZ2) ",1]
[{"$nulls":3},"Dell PowerStore 1200 T - EMEA",1]
[{"$nulls":5},"PowerStore 1200","GABW73H","PowerStore 1200T Base Dell Customer Racked TLA","[210-BCZK]",1]
[{"$nulls":5},"Memory Capacity","G58PSGD","384GB Appliance DIMM (192GB Per Node)","[370-AEZP]",1]
[{"$nulls":5},"DRR (Used for Internal Data Tracking)","GCUT7NJ",0.12569444444444444,"[379-BEIQ]",1]
[{"$nulls":5},"Drives","GT6URWQ","15.36TB NVMe SSD (High Capacity Array) TLA","[400-BQGF]",15]
[{"$nulls":5},"Operating Environment","GLC6HFV","TLA HW Only Order","[379-BDUU]",1]
[{"$nulls":5},"4 Port Mezz Cards","GP59QJZ","25GBE Optical 4 Port Card Pair (SFPs not included)","[406-BBOO]",1]
[{"$nulls":5},"Optional Appliance IO Module","GSCX3RP","32GB FC 4 Port IO Module Pair (SFPs included)","[565-BBJS]",1]
[{"$nulls":5},"Power Supply","GOQ271R","Dual 1800W (200-240V) Lot 9 Power Supply , includes C13/C14 Power Cords","[450-BBBJ]",1]
[{"$nulls":5},"Cable Pairs","GFKM8N4","3M Passive 25G Twinax Cable QTY 2","[470-ADUI]",4]
[{"$nulls":5},"Install Kits","GP49UY5","PowerStore Base Enclosure Install Kit","[343-BBTN]",1]
[{"$nulls":5},"NVRAM Caching Device","G0A32UK","PowerStore NVRAM FIPS QTY 2","[400-BOBK]",1]
[{"$nulls":5},"Dell Services: Hardware Support","G6JLC01","Parts Only Warranty 36Months, 36 Month(s)","[709-BDKZ]",1]
[{"$nulls":5},"Dell Services: Extended Service","GM6395C","Prosupport Plus and 4Hr Mission Critical, 60 Month(s)","[199-BJJO], [199-BJJP]",1]
[{"$nulls":5},"Storage Configuration","GIY80C2","Single Appliance","[800-BBQV]",1]
[{"$nulls":5},"Dell Services:Deployment Services","G4YRE2B","ProDeploy Plus for PowerStore 1xxx T","[683-23387], [706-12528]",1]
[{"$nulls":5},"Dell Services:Additional Deployment Services","GY4R9AF","ProDeploy Plus Add-On for PowerStore Remote Replication (Requires ProDeploy Plus)","[519-10199]",1]
[{"$nulls":5},"Dell Services:Additional Deployment Services","GG6179R","ProDeploy Plus Add-On for PowerStore Local Protection (Requires ProDeploy Plus)","[519-10194]",1]
[{"$nulls":5},"Data Migration Services","G7WJPUC","Data Migration Services: Remote Virtual V2V Migration 101 Plus VMs (Per VM)","[519-12227]",135]
[{"$nulls":3},"Metro node for PowerStore  EMEA",2]
[{"$nulls":5},"Dell EMC metro node","G7ZD5CJ","Metro node Base Configuration","[210-AXRR], [321-BCYJ], [329-BDMR], [330-BBGN], [350-BBKB], [350-BCCT], [370-AAIP], [370-AEVR], [379-BCQW], [379-BCQY], [379-BDCO], [384-BBQJ], [385-BBKT], [405-AACD], [429-ABBF], [450-AAGG], [450-AJSC], [461-AADZ], [540-BBVO], [555-BCKP], [605-BBFN], [623-BBDW], [631-AACK], [631-ACTH], [770-BCIO], [780-BCDM], [800-BBDM]",1]
[{"$nulls":5},"Fibre Channel Adapters","G7HFQLN","Emulex LPE 35002 Dual Port 32Gb Fibre Channel HBA, PCIe Low Profile","[406-BBMO]",2]
[{"$nulls":5},"Hard Drives","G3ZJM0K","480GB SSD SATA Read Intensive 6Gbps 512 2.5in Hot-plug AG Drive, 1 DWPD","[400-AXTV]",1]
[{"$nulls":5},"Optics","G0FVJIE","SFP+ SR Optic, 10GbE, for all SFP+ ports except high temp validation warning cards","[407-BCBE]",2]
[{"$nulls":5},"Memory DIMM","GQ3BS0I","16GB RDIMM, 3200MT/s, Dual Rank","[370-AEVQ]",4]
[{"$nulls":5},"Processor","GS1G2MP","Intel Xeon Silver 4208 2.1G, 8C/16T, 9.6GT/s, 11M Cache, Turbo, HT (85W) DDR4-2400","[338-BSWX]",2]
[{"$nulls":5},"Processor Thermal Configuration",5099793,"Standard Heatsink for 2 CPU","[370-ABWE], [412-AAIQ], [412-AAIQ]",1]
[{"$nulls":5},"Brand Kit","GKHZXQ0","Bezel and Luggage Tag for PowerStore","[325-BDZP], [350-BCDY]",1]
[{"$nulls":5},"Cable Management Arm Kit","G4PAORU","CMA KIT (PWR,LCOM,MGMT Cables Included)","[470-AENQ]",1]
[{"$nulls":5},"Dell Services: Hardware Support","G0NZD1S","Basic Next Business Day 36Months, 36 Month(s)","[709-BDRR]",1]
[{"$nulls":5},"Dell Services: Extended Service","GBUE8WV","ProSupport Plus and 4Hr Mission Critical, 60 Month(s)","[199-BJXL], [199-BJXM]",1]
[{"$nulls":5},"Metro node Operating System","GFQ6SOY","Metro node Operating System","[528-CNOH]",1]
[{"$nulls":5},"Local Capacity License","GCSM8YX","Local 10TB Capacity License","[528-CNPF]",1]
[{"$nulls":5},"Software Services - Metro node Local Base Capacity","GNX103T","ProSupport Plus Mission Critical metro node Local Base Incl 10TB Software Support-Maint, 60 Month(s)","[487-BGNT]",1]
[{"$nulls":5},"Dell Services: Deployment Services","G8QMLNH","ProDeploy Plus for Metro Node Single Node  Deployment","[683-26310], [706-12529]",1]
[{"$nulls":5},"Shipping Material","GQPW7FK","PowerEdge R640 x8 Drive Shipping Material","[340-COPS]",1]
[{"$nulls":5},"Regulatory","G27VF4L","PowerEdge R640 CE,CCC,BIS Marking","[389-DTIV]",1]
[{"$nulls":5},"Shipping","GBIHPJ4","Metro node Shipping EMEA1","[340-CUXV]",1]
[{"$nulls":3},"Metro node Software for PowerStore  EMEA",1]
[{"$nulls":5},"Metro node Software","GR8PWBT","Metro node Software","[210-AYIY]",1]
[{"$nulls":5},"Hardware Selection","GA217I9","PowerStore","[800-BBQV]",1]
[{"$nulls":5},"Metro node Powerstore Frame License","GGJY7DR","Metro node PowerStore 1K METRO FB SW","[528-CNNT]",1]
[{"$nulls":5},"Software Services : Perpetual (VP)","G2TX1H3","ProSupport Plus Mission Critical metro node Software Support-Maintenance, 60 Month(s)","[487-BGJY]",1]
[{"$nulls":3},"Metro node Deployment Services - EMEA",1]
[{"$nulls":5},"Metro node Deployment Services","G5L4CX2","Metro node Deployment Services","[210-BBCB]",1]
[{"$nulls":5},"Add-On Services for ProDeploy","GFGWRS5","ProDeploy Plus Add-On:  Metro Node Witness Module (Requires ProDeploy Plus)","[519-12568]",1]
[{"$nulls":3},"Dell EMC AppSync for PowerStore - EMEA",1]
[{"$nulls":5},"Appsync for PowerStore","GB81KRV","AppSync for PowerStore","[210-BEGM]",1]
[{"$nulls":5},"Deployment Services",57261,"No Installation Service Selected (Contact Sales rep for more details)","[683-11930]",1]
[{"$nulls":5},"AppSync Software","GQ70RAI","AppSync Str Pk for PowerStore","[528-BYHF]",1]
[{"$nulls":5},"Sftwr Svcs - Perpetual","G5F3N98","ProSupport Plus Mission Critical Appsync for PowerStore Sftwr Spt-Maint, 60 Month(s)","[487-BJQM]",1]
[{"$nulls":3},"Connectrix DS-6620B MidRange Cosell",2]
[{"$nulls":5},"Connectrix DS-6620B","GAWJUZ0","DS-6620B 24P/48P V2 switch (FOS 9.0 min) w/front-to-rear airflow (includes 24x32Gb SFPs a","[210-AZLG]",1]
[{"$nulls":5},"Dell Services: Hardware Support","G5COX36","Parts Only Warranty 36Months, 36 Month(s)","[709-BDSY]",1]
[{"$nulls":5},"Dell Services: Extended Service","GTWKL3Y","ProSupport Plus and 4Hr Mission Critical, 60 Month(s)","[199-BJSW], [199-BJSX]",1]
[{"$nulls":5},"Dell Services: Deployment Services","G26UVJX","ProDeploy Plus Connectrix Fibre Channel Switch (up to 4 new hosts)","[683-23121], [683-23122], [706-12472]",1]
[{"$nulls":5},"MultiMode Fiber LC/LC patch cables","GBFV6RW","OM4 LC/LC Multi Mode Fiber Cable (optics required), 5 Meter","[407-BCQM]",12]
[{"$nulls":5},"MultiMode Fiber LC/LC patch cables","G9L1FGK","OM4 LC/LC Multi Mode Fiber Cable (optics required), 10 Meter","[407-BCQH]",12]
[{"$nulls":5},"Power Cords","GN3XZY2","QTY 2 Connectrix C14-TO-C13 3M INTERNAL CAB POWER CORDS-B","[450-ABLX]",1]
[null,"Group 1","4242639.9.1","EMC_POWERSTORET_GEN2_EMEA_2 (CPT) ",1]
[{"$nulls":3},"Dell PowerStore 1200 T - EMEA",1]
[{"$nulls":5},"PowerStore 1200","GABW73H","PowerStore 1200T Base Dell Customer Racked TLA","[210-BCZK]",1]
[{"$nulls":5},"Memory Capacity","G58PSGD","384GB Appliance DIMM (192GB Per Node)","[370-AEZP]",1]
[{"$nulls":5},"DRR (Used for Internal Data Tracking)","GCUT7NJ",0.12569444444444444,"[379-BEIQ]",1]
[{"$nulls":5},"Drives","GT6URWQ","15.36TB NVMe SSD (High Capacity Array) TLA","[400-BQGF]",15]
[{"$nulls":5},"Operating Environment","GLC6HFV","TLA HW Only Order","[379-BDUU]",1]
[{"$nulls":5},"4 Port Mezz Cards","GP59QJZ","25GBE Optical 4 Port Card Pair (SFPs not included)","[406-BBOO]",1]
[{"$nulls":5},"Optional Appliance IO Module","GSCX3RP","32GB FC 4 Port IO Module Pair (SFPs included)","[565-BBJS]",1]
[{"$nulls":5},"Power Supply","GOQ271R","Dual 1800W (200-240V) Lot 9 Power Supply , includes C13/C14 Power Cords","[450-BBBJ]",1]
[{"$nulls":5},"Cable Pairs","GFKM8N4","3M Passive 25G Twinax Cable QTY 2","[470-ADUI]",4]
[{"$nulls":5},"Install Kits","GP49UY5","PowerStore Base Enclosure Install Kit","[343-BBTN]",1]
[{"$nulls":5},"NVRAM Caching Device","G0A32UK","PowerStore NVRAM FIPS QTY 2","[400-BOBK]",1]
[{"$nulls":5},"Dell Services: Hardware Support","G6JLC01","Parts Only Warranty 36Months, 36 Month(s)","[709-BDKZ]",1]
[{"$nulls":5},"Dell Services: Extended Service","GM6395C","Prosupport Plus and 4Hr Mission Critical, 60 Month(s)","[199-BJJO], [199-BJJP]",1]
[{"$nulls":5},"Storage Configuration","GIY80C2","Single Appliance","[800-BBQV]",1]
[{"$nulls":5},"Dell Services:Deployment Services","G4YRE2B","ProDeploy Plus for PowerStore 1xxx T","[683-23387], [706-12528]",1]
[{"$nulls":5},"Dell Services:Additional Deployment Services","GY4R9AF","ProDeploy Plus Add-On for PowerStore Remote Replication (Requires ProDeploy Plus)","[519-10199]",1]
[{"$nulls":5},"Dell Services:Additional Deployment Services","GG6179R","ProDeploy Plus Add-On for PowerStore Local Protection (Requires ProDeploy Plus)","[519-10194]",1]
[{"$nulls":5},"Data Migration Services","G7WJPUC","Data Migration Services: Remote Virtual V2V Migration 101 Plus VMs (Per VM)","[519-12227]",135]
[{"$nulls":3},"Dell EMC AppSync for PowerStore - EMEA",1]
[{"$nulls":5},"Appsync for PowerStore","GB81KRV","AppSync for PowerStore","[210-BEGM]",1]
[{"$nulls":5},"Deployment Services",57261,"No Installation Service Selected (Contact Sales rep for more details)","[683-11930]",1]
[{"$nulls":5},"AppSync Software","GQ70RAI","Original Equipment Manufacturer ","[528-BYHF]",1]
[{"$nulls":5},"Sftwr Svcs - Perpetual","G5F3N98","ProSupport Plus Mission Critical Appsync for PowerStore Sftwr Spt-Maint, 60 Month(s)","[487-BJQM]",1]
[{"$nulls":3},"Connectrix DS-6620B MidRange Cosell",2]
[{"$nulls":5},"Connectrix DS-6620B","GAWJUZ0","DS-6620B 24P/48P V2 switch (FOS 9.0 min) w/front-to-rear airflow (includes 24x32Gb SFPs a","[210-AZLG]",1]
[{"$nulls":5},"Dell Services: Hardware Support","G5COX36","Parts Only Warranty 36Months, 36 Month(s)","[709-BDSY]",1]
[{"$nulls":5},"Dell Services: Extended Service","GTWKL3Y","ProSupport Plus and 4Hr Mission Critical, 60 Month(s)","[199-BJSW], [199-BJSX]",1]
[{"$nulls":5},"Dell Services: Deployment Services","G26UVJX","ProDeploy Plus Connectrix Fibre Channel Switch (up to 4 new hosts)","[683-23121], [683-23122], [706-12472]",1]
[{"$nulls":5},"MultiMode Fiber LC/LC patch cables","GBFV6RW","OM4 LC/LC Multi Mode Fiber Cable (optics required), 5 Meter","[407-BCQM]",12]
[{"$nulls":5},"MultiMode Fiber LC/LC patch cables","G9L1FGK","OM4 LC/LC Multi Mode Fiber Cable (optics required), 10 Meter","[407-BCQH]",12]
[{"$nulls":5},"Power Cords","GN3XZY2","QTY 2 Connectrix C14-TO-C13 3M INTERNAL CAB POWER CORDS-B","[450-ABLX]",1]
[null,"Group 1","4242639.9.1","PowerEdge R450 - Full Configuration - [EMEA_R450] - Metro Witness Server Witness Server ",1]
[{"$nulls":5},"Base","GJFZ58P","PowerEdge R450 Server","[210-AZDS]",1]
[{"$nulls":5},"FRONT STORAGE","G6VIQUW","Chassis with up to 8x2.5\" Drives","[379-BDTF]",1]
[{"$nulls":5},"BACKPLANE","GK0E3OX","SAS/SATA Backplane","[379-BDSS]",1]
[{"$nulls":5},"Trusted Platform Module","GGX1VDO","Trusted Platform Module 2.0 V3","[461-AAIG]",1]
[{"$nulls":5},"Chassis Configuration","G6R7ZNG","2.5\" Chassis with up to 8 Hard Drives (SAS/SATA) 1 CPU","[321-BGQS]",1]
[{"$nulls":5},"Processor","GGK2I89","Intel® Xeon® Silver 4314 2.4G, 16C/32T, 10.4GT/s, 24M Cache, Turbo, HT (135W) DDR4-2666","[338-CBWK]",1]
[{"$nulls":5},"Additional Processor","GWSO9LE","No Additional Processor","[374-BBBX]",1]
[{"$nulls":5},"Processor Thermal Configuration","GLEMU9G","Heatsink for 1 CPU configuration (CPU less or equal 165W)","[412-AAVV], [412-ABBC]",1]
[{"$nulls":5},"Memory Configuration Type","GH9QBEI","Performance Optimized","[370-AAIP]",1]
[{"$nulls":5},"Memory DIMM Type and Speed","GR3CFNV","3200MT/s RDIMMs","[370-AEVR]",1]
[{"$nulls":5},"Memory Capacity","GQ3BS0I","16GB RDIMM, 3200MT/s, Dual Rank","[370-AEVQ]",4]
[{"$nulls":5},"RAID Configuration","GOV1697","C3, RAID 1 for 2 HDDs or SSDs (Matching Type/Speed/Capacity)","[780-BCDN]",1]
[{"$nulls":5},"RAID/Internal Storage Controllers","GGQ3MK6","Front PERC H745 Front Load","[405-AAUZ], [750-ACFR]",1]
[{"$nulls":5},"Hard Drives","G3ZJM0K","480GB SSD SATA Read Intensive 6Gbps 512 2.5in Hot-plug AG Drive, 1 DWPD","[400-AXTV]",2]
[{"$nulls":5},"BIOS and Advanced System Configuration Settings","GEARJ9V","Power Saving BIOS Setting","[384-BBBH]",1]
[{"$nulls":5},"Embedded Systems Management (Multi)","G9X14RE","Server Secured Component Verification","[528-COYT]",1]
[{"$nulls":5},"Embedded Systems Management (Multi)","GE3OWU1","iDRAC9, Express 15G","[385-BBQZ]",1]
[{"$nulls":5},"Fans","GH14MID","Standard Fan x7","[384-BCTN]",1]
[{"$nulls":5},"Power Supply","GLYN2J7","Dual, Hot-plug, Power Supply Fully Redundant (1+1), 800W, Mixed Mode, NAF","[450-AIQX]",1]
[{"$nulls":5},"Power Cords","GDE0CHU","Rack Power Cord 2M (C13/C14 10A)","[450-AADY]",2]
[{"$nulls":5},"PCIe Riser","GB8I5NQ","Riser Config 0, 1xOCP 3.0(x16)+ 1x16LP","[330-BBVF]",1]
[{"$nulls":5},"Motherboard","G65L43K","PowerEdge R450 Motherboard with Broadcom 5720 Dual Port 1Gb On-Board LOM, V4","[329-BHNE]",1]
[{"$nulls":5},"OCP 3.0 Network Adapters","G81KH5Z","Broadcom 57412 Dual Port 10GbE SFP+, OCP NIC 3.0","[540-BCNT]",1]
[{"$nulls":5},"Quick Sync","GT8Y6M9","No Quick Sync","[350-BCEM]",1]
[{"$nulls":5},"Password","G2T768J","iDRAC,Factory Generated Password","[379-BCSF]",1]
[{"$nulls":5},"Group Manager","GTVA94K","iDRAC Group Manager, Disabled","[379-BCQY]",1]
[{"$nulls":5},"Bezel","G0PNWIK","Standard Bezel for x8 Chassis","[325-BCHH], [350-BCFL]",1]
[{"$nulls":5},"Optics & Cables for Network Cards","G0FVJIE","SFP+ SR Optic, 10GbE, for all SFP+ ports except high temp validation warning cards","[407-BCBE]",2]
[{"$nulls":5},"Operating System","G78MU35","No Operating System","[611-BBBF]",1]
[{"$nulls":5},"OS Media Kits","GKH7AZI","No Media Required","[605-BBFN]",1]
[{"$nulls":5},"Rack Rails","GFK9A8H","ReadyRails™ Static Rails for 2/4-post Racks","[770-BBBM]",1]
[{"$nulls":5},"Internal Optical Drive","GZP2ROB","No Internal Optical Drive","[429-AAIQ]",1]
[{"$nulls":5},"System Documentation","GVRYSM7","No Systems Documentation, No OpenManage DVD Kit","[631-AACK]",1]
[{"$nulls":5},"SHIPPING","G1RX69D","PowerEdge R450 Shipping EMEA1 (English/French/German/Spanish/Russian/Hebrew)","[340-CWXJ]",1]
[{"$nulls":5},"Shipping Material","G3SIGC1","PowerEdge R450 x8 Short Drive Shipping Material","[343-BBRQ]",1]
[{"$nulls":5},"Regulatory","GIDYS8Z","PowerEdge 1U CE, CCC, Marking, No BIS Marking","[389-EBNS], [389-EBNV]",1]
[{"$nulls":5},"Services: Hardware Support","G2L3ABJ","Basic Next Business Day 36 Months, 36 Month(s)","[709-BBIL]",1]
[{"$nulls":5},"Services: Extended Service","GU08IG4","ProSupport Plus and Next Business Day Onsite Service, 60 Month(s)","[865-BBND], [865-BBNE]",1]
[{"$nulls":5},"Dell Services: Deployment Services",959563,"ProDeploy Plus Dell Server R Series 1U/2U","[683-19204], [683-19205], [706-12474]",1]
[{"$nulls":5},"Anti Theft Device & Asset Tagging","G2K1LTI","Asset Tag - ProSupport (Website, barcode, Onboard MacAddress)","[293-10025]",1]
[{"$nulls":5},"Configuration Services Asset Report","GL8CKHO","Configuration Services, Standard ISG System Report, Deliver Via Email","[708-10082]",1]
[{"$nulls":5},"Shipping Box Labels - Standard","GDZ0XTY","Order Configuration Shipbox Label (Ship Date, Model, Processor Speed, HDD Size, RAM)","[293-10049]",1]
[{"$nulls":11},{"$f":"SUM(L9:L710)","v":{"v":0,"d":"R0.00"}},{"$f":"SUM(M9:M710)","v":{"v":0,"d":"R0.00"}}]
[]
[{"$nulls":5},"Dell Software TLA"]
[]
[{"$nulls":5},"Product",null,"Licensed SW","License Model","Qty"]
[{"$nulls":5},"PowerStore TLA Software",null,"PowerStore 1200 Base License TLA=IC ","147-BCVE",5]
[{"$nulls":5},"Base Capacity Software",null,"PowerStore Capacity SW TLA=CB ","147-BBKO",742]
[{"$nulls":5},"Service",null,"Service Sftwr Svcs - TLA ProSupport Plus Mission Critical PowerStore-TLA Sftwr Spt-Maint, 60 Month(s) ","487-BJFQ",1]
[{"$nulls":5},"Base",null,"VxRail SW only Virtual Base TLA","210-BEOP",1]
[{"$nulls":5},"Vxrail HCI System Software Processor",null,"VxRail HCI15G AF/Hybrid ProcrGold TLA=IG ","147-BCSW",35]
[{"$nulls":5},"Vxrail HCI System Software Processor",null,"VxRail 15G DynNode Processor Plat TLA=IG ","147-BCTG",44]
[{"$nulls":5},"VxRail HCI System Software Capacity Drive",null,"VxRail HCI Sys SW (CAP3.84 SATA)TLA=CF ","147-BCTM",70]
[{"$nulls":5},"VxRail HCI System Software Memory",null,"VxRail HCI Sys Memory 32GB TLA=CG ","147-BCSY",633]
[{"$nulls":5},"VxRail HCI System Software Memory",null,"VxRail HCI Sys Memory 64GB TLA=CG ","147-BCSP",352]
[{"$nulls":5},"Service",null,"Service Sftwr Svcs - TLA ProSupport Plus Mission Critical VxRail AF-TLA Sftwr Spt-Maint, 60 Month(s) ","487-BJLD",1]

{"sheet":"VMwarePricing Schedule","index":1,"n_rows":16,"n_cols":7,"rows_kept":16,"merged":[[1,4,6,4],[1,5,6,5],[1,6,6,6],[7,0,11,0],[7,2,11,2],[7,4,11,4],[7,5,11,5],[7,6,11,6],[12,4,14,4],[12,5,14,5],[12,6,14,6]]}
["Item","Description","Item","Description",null,"Price Excluding VAT","Price Including VAT"]
[null,"Based on the consumption model, the solution includes the below.",null,"Based on the consumption model, the solution includes the below.",null,{"v":0,"d":"R0.00"},{"v":0,"d":"R0.00"}]
["VMware Private Cloud Platform","1.       vSphere Enterprise Plus","VMware Private Cloud Platform","1.       vSphere Enterprise Plus"]
[null,"2.       vCenter standard",null,"2.       vCenter standard"]
[null,"3.       NSX Prof",null,"3.       NSX Prof"]
[null,"4.       vRealize Operations Manager adv",null,"4.       vRealize Operations Manager adv"]
[null,"5.       Site Recovery Manager",null,"5.       Site Recovery Manager"]
["Value Added Services","The below services are included:","Value Added Services","The below services are included:","Delivered  by VMware Cloud Service Providers"]
[null,"1.       Install, Manage & Operate VMware Software delivered to the customer as a Service.",null,"1.       Install, Manage & Operate VMware Software delivered to the customer as a Service."]
[null,"2.       Metering and reporting of VMware Product Usage and monthly billing to end customers. ",null,"2.       Metering and reporting of VMware Product Usage and monthly billing to end customers. "]
[null,"3.       First-level support to customers & Log Support Calls to VMware.",null,"3.       First-level support to customers & Log Support Calls to VMware."]
[]
["Deployment: ","These are services to stabilize and bring to a supported state the VMware environment for National Treasury. ","Deployment: ","These are services to stabilize and bring to a supported state the VMware environment for National Treasury. ","National Treasury To Determine based on previous SOW."]
["(Including Migrations and Upgrades)",null,"(Including Migrations and Upgrades)"]
[null,"Note: The previous scope can be used for this, based on the previous RFP",null,"Note: The previous scope can be used for this, based on the previous RFP"]
[{"$nulls":5},{"$f":"SUM(F2:F15)","v":{"v":0,"d":"R0.00"}},{"$f":"SUM(G2:G15)","v":{"v":0,"d":"R0.00"}}]

{"sheet":"Prof Services Pricing schedule","index":2,"n_rows":15,"n_cols":5,"rows_kept":15,"merged":[[4,0,4,2],[5,0,5,2],[6,0,6,2],[7,0,7,2],[9,0,9,2],[10,0,10,2],[11,0,11,2],[12,0,12,2],[13,0,13,2]]}
[]
[]
[]
[]
["Year1 Professional Services",null,null,"Price Excl VAT","Price Including VAT"]
["5yrs - Managed Services -  24x7 Hybrid : (Onsite Resources during business hrs & Remote after hrs) - Yearly Price",null,null,{"v":0,"d":"R0.00"},{"v":0,"d":"R0.00"}]
["Deployment of VCF Components & SRM (Once Off)                                   ",null,null,{"v":0,"d":"R0.00"},{"v":0,"d":"R0.00"}]
[{"$nulls":3},{"$f":"SUM(D6:D7)","v":{"v":0,"d":"R0.00"}},{"$f":"SUM(E6:E7)","v":{"v":0,"d":"R0.00"}}]
[]
["Year2 to Year 5 Services",null,null,"Price Excl VAT","Price Including VAT"]
["Year 2 Managed Services -  24x7 Hybrid : (Onsite Resources during business hrs & Remote after hrs) - Yearly Price"]
["Year 3 Managed Services -  24x7 Hybrid : (Onsite Resources during business hrs & Remote after hrs) - Yearly Price"]
["Year 3 Managed Services -  24x7 Hybrid : (Onsite Resources during business hrs & Remote after hrs) - Yearly Price"]
["Year 5 Managed Services -  24x7 Hybrid : (Onsite Resources during business hrs & Remote after hrs) - Yearly Price"]
[{"$nulls":3},{"$f":"SUM(D11:D14)","v":{"v":0,"d":"R0.00"}},{"$f":"SUM(E11:E14)","v":{"v":0,"d":"R0.00"}}]